#

##

##

##

##

##

##

    猩ision Build Log
    Tool Versions:
    IDE-Version: 米Vision V5.28.0.0
    Copyright (C) 2019 ARM Ltd and ARM Germany GmbH. All rights reserved.
    License Information: HAHA Markin, HAHA, LIC=VGXG8-3CKFQ-63XMB-246PQ-J4CUG-RTS7K

    Tool Versions:
    Toolchain:       MDK-ARM Plus  Version: 5.28.0.0
    Toolchain Path:  C:\Keil_v5\ARM\ARMCC\Bin
    C Compiler:      Armcc.exe V5.06 update 6 (build 750)
    Assembler:       Armasm.exe V5.06 update 6 (build 750)
    Linker/Locator:  ArmLink.exe V5.06 update 6 (build 750)
    Library Manager: ArmAr.exe V5.06 update 6 (build 750)
    Hex Converter:   FromElf.exe V5.06 update 6 (build 750)
    CPU DLL:         SARMCM3.DLL V5.28.0.0
    Dialog DLL:      DARMCM1.DLL V1.19.2.0
    Target DLL:      UL2CM3.DLL V1.162.16.0
    Dialog DLL:      TARMCM1.DLL V1.14.1.0

    Project:
    D:\Custom\斐陓\WL668_Pixel 6 A_CSOT6_ICNA3511A_ CST6656S_OLED\覃彸測鎢\WL668T_GOOGLE_P6A_S47_CSOT6.0_ICNA3511A_OLED_FHD_20231227\WL668T_GOOGLE_P6A_S47_CSOT6.0_ICNA3511A_OLED_FHD_20231227\project\WL668T\WL668T.uvprojx
    Project File Date:  02/02/2024

    Output:
    *** Using Compiler 'V5.06 update 6 (build 750)', folder: 'C:\Keil_v5\ARM\ARMCC\Bin'
    Rebuild target 'WL668T'
    creating preprocessor file for main.c...
    compiling main.c...
    creating preprocessor file for p6a_demo.c...
    compiling p6a_demo.c...
    ..\..\src\app\P6A\p6a_demo.c(131): warning:  #550-D: variable "sg_exit_idle_mode_flag"  was set but never used
      static bool sg_exit_idle_mode_flag = false;
    ..\..\src\app\P6A\p6a_demo.c(134): warning:  #177-D: variable "pps_renew_flag"  was declared but never referenced
      static uint32_t pps_renew_flag = 0;
    ..\..\src\app\P6A\p6a_demo.c(135): warning:  #177-D: variable "pwr_rst_flag"  was declared but never referenced
      static uint32_t pwr_rst_flag = 0;
    ..\..\src\app\P6A\p6a_demo.c(404): warning:  #177-D: variable "reg53_E8_fg"  was declared but never referenced
      static bool reg53_E8_fg=0;
    ..\..\src\app\P6A\p6a_demo.c(483): warning:  #177-D: function "ap_dcs_set_exit_idle_mode"  was declared but never referenced
      static bool ap_dcs_set_exit_idle_mode(hal_dsi_rx_ctrl_handle_t *handler, hal_dcs_packet_t *dcs_packet)
    ..\..\src\app\P6A\p6a_demo.c(508): warning:  #177-D: function "soft_te_timer_init"  was declared but never referenced
      static void soft_te_timer_init()
    ..\..\src\app\P6A\p6a_demo.c(522): warning:  #177-D: function "ap_dcs_set_frame_change"  was declared but never referenced
      static bool ap_dcs_set_frame_change(hal_dsi_rx_ctrl_handle_t *handler, hal_dcs_packet_t *dcs_packet)
    ..\..\src\app\P6A\p6a_demo.c(541): warning:  #177-D: function "ap_set_FPS_B1"  was declared but never referenced
      static bool ap_set_FPS_B1(hal_dsi_rx_ctrl_handle_t *handler, hal_dcs_packet_t *dcs_packet)
    ..\..\src\app\P6A\p6a_demo.c: 8 warnings, 0 errors
    creating preprocessor file for board.c...
    compiling board.c...
    assembling startup_ARMCM0.s...
    linking...
    Program Size: Code=50220 RO-data=976 RW-data=920 ZI-data=11632
    FromELF: creating hex file...
    After Build - User command #1: fromelf  --bin  -o  .\Objects\WL668T_P6A_S47_CSOT6_ICNA3511A_20240202.bin  .\Objects\WL668T_P6A_S47_CSOT6_ICNA3511A_20240202.axf
    ".\Objects\WL668T_P6A_S47_CSOT6_ICNA3511A_20240202.axf" - 0 Error(s), 8 Warning(s).

    Software Packages used:

    Package Vendor: ARM
                    http://www.keil.com/pack/ARM.CMSIS.5.5.1.pack
                    ARM.CMSIS.5.5.1
                    CMSIS (Cortex Microcontroller Software Interface Standard)
       * Component: CORE Version: 5.2.0

    Collection of Component include folders:
      .\RTE\_WL668T
      C:\Users\Markin\AppData\Local\Arm\Packs\ARM\CMSIS\5.5.1\CMSIS\Core\Include
      C:\Users\Markin\AppData\Local\Arm\Packs\ARM\CMSIS\5.5.1\Device\ARM\ARMCM0\Include

    Collection of Component Files used:

       * Component: ARM::CMSIS:CORE:5.2.0
    Build Time Elapsed:  00:00:02