Component: ARM Compiler 5.06 update 6 (build 750) Tool: armlink [4d35ed]

==============================================================================

Section Cross References

    main.o(i.main) refers to board.o(i.board_Init) for board_Init
    main.o(i.main) refers to p6a_demo.o(i.google_p6a_demo) for google_p6a_demo
    main.o(i.main) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.Gpio_swire_output) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    p6a_demo.o(i.Gpio_swire_output) refers to tau_delay.o(i.delayMs) for delayMs
    p6a_demo.o(i.Gpio_swire_output) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    p6a_demo.o(i.Gpio_swire_output) refers to tau_delay.o(i.delayUs) for delayUs
    p6a_demo.o(i.Panel_CCM) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) for hal_dsi_tx_ctrl_set_ccm
    p6a_demo.o(i.REG_51_OFF_output) refers to idiv.o(.text) for __aeabi_idivmod
    p6a_demo.o(i.REG_51_OFF_output) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    p6a_demo.o(i.REG_51_OFF_output) refers to tau_delay.o(i.delayMs) for delayMs
    p6a_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) for hal_dsi_rx_ctrl_send_ack_cmd
    p6a_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) for hal_dsi_rx_ctrl_get_max_ret_size
    p6a_demo.o(i.ap_dcs_read) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.ap_dcs_read) refers to p6a_demo.o(.data) for g_rx_ctrl_handle
    p6a_demo.o(i.ap_dcs_set_backlight) refers to idiv.o(.text) for __aeabi_idivmod
    p6a_demo.o(i.ap_dcs_set_backlight) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    p6a_demo.o(i.ap_dcs_set_backlight) refers to p6a_demo.o(.data) for rd_51_val
    p6a_demo.o(i.ap_dcs_set_display_off) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    p6a_demo.o(i.ap_dcs_set_display_off) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.ap_dcs_set_display_off) refers to p6a_demo.o(.data) for panel_display_done
    p6a_demo.o(i.ap_dcs_set_display_on) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) for hal_dsi_rx_ctrl_pre_init_pps
    p6a_demo.o(i.ap_dcs_set_display_on) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) for hal_dsi_rx_ctrl_toggle_resolution
    p6a_demo.o(i.ap_dcs_set_display_on) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.ap_dcs_set_display_on) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    p6a_demo.o(i.ap_dcs_set_display_on) refers to p6a_demo.o(.data) for g_resolution_change
    p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode) for hal_dsi_tx_ctrl_set_tear_mode
    p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to tau_delay.o(i.delayMs) for delayMs
    p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to hal_swire.o(i.hal_swire_enable) for hal_swire_enable
    p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to p6a_demo.o(.data) for g_tx_ctrl_handle
    p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to p6a_demo.o(i.ap_rstn_pull_down_cb) for ap_rstn_pull_down_cb
    p6a_demo.o(i.ap_dcs_set_exit_idle_mode) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) for hal_dsi_rx_ctrl_set_hw_cmd_filter
    p6a_demo.o(i.ap_dcs_set_exit_idle_mode) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.ap_dcs_set_exit_idle_mode) refers to p6a_demo.o(.data) for sg_exit_idle_mode_flag
    p6a_demo.o(i.ap_dcs_set_exit_sleep_mode) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.ap_dcs_set_frame_change) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode) for hal_dsi_tx_ctrl_set_tear_mode
    p6a_demo.o(i.ap_dcs_set_frame_change) refers to p6a_demo.o(.data) for g_tx_ctrl_handle
    p6a_demo.o(i.ap_rstn_pull_down_cb) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.ap_rstn_pull_down_cb) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    p6a_demo.o(i.ap_rstn_pull_down_cb) refers to p6a_demo.o(.data) for sg_system_suspend
    p6a_demo.o(i.ap_rstn_pull_high_cb) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    p6a_demo.o(i.ap_rstn_pull_high_cb) refers to p6a_demo.o(.data) for sg_system_resume
    p6a_demo.o(i.ap_set_FPS_B1) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    p6a_demo.o(i.app_display_init) refers to p6a_demo.o(i.app_mipi_rx_init) for app_mipi_rx_init
    p6a_demo.o(i.app_display_init) refers to hal_pwr.o(i.hal_pwr_get_vcc_power_ready) for hal_pwr_get_vcc_power_ready
    p6a_demo.o(i.app_display_init) refers to p6a_demo.o(i.app_gpio_init) for app_gpio_init
    p6a_demo.o(i.app_display_init) refers to hal_swire.o(i.hal_swire_init) for hal_swire_init
    p6a_demo.o(i.app_display_init) refers to hal_swire.o(i.hal_swire_set_timer) for hal_swire_set_timer
    p6a_demo.o(i.app_display_init) refers to p6a_demo.o(i.app_mipi_tx_init) for app_mipi_tx_init
    p6a_demo.o(i.app_display_init) refers to p6a_demo.o(i.app_mipi_tx_start) for app_mipi_tx_start
    p6a_demo.o(i.app_gpio_init) refers to hal_gpio.o(i.hal_gpio_config_pad) for hal_gpio_config_pad
    p6a_demo.o(i.app_gpio_init) refers to p6a_demo.o(.constdata) for .constdata
    p6a_demo.o(i.app_init_panel) refers to p6a_demo.o(i.app_tx_panel_reset) for app_tx_panel_reset
    p6a_demo.o(i.app_init_panel) refers to p6a_demo.o(i.send_panel_init_code) for send_panel_init_code
    p6a_demo.o(i.app_init_panel) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    p6a_demo.o(i.app_init_panel) refers to tau_delay.o(i.delayMs) for delayMs
    p6a_demo.o(i.app_init_panel) refers to hal_swire.o(i.hal_swire_enable) for hal_swire_enable
    p6a_demo.o(i.app_init_panel) refers to hal_swire.o(i.hal_swire_set_pulse) for hal_swire_set_pulse
    p6a_demo.o(i.app_init_panel) refers to p6a_demo.o(.constdata) for panel_init_code
    p6a_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) for hal_dsi_rx_ctrl_create_handle
    p6a_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) for hal_dsi_rx_ctrl_pre_init_pps
    p6a_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    p6a_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    p6a_demo.o(i.app_mipi_rx_init) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.app_mipi_rx_init) refers to p6a_demo.o(.data) for g_rx_ctrl_handle
    p6a_demo.o(i.app_mipi_rx_init) refers to p6a_demo.o(.constdata) for g_cus_rx_dcs_execute_table
    p6a_demo.o(i.app_mipi_rx_init) refers to p6a_demo.o(i.ap_dcs_read) for ap_dcs_read
    p6a_demo.o(i.app_mipi_rx_init) refers to p6a_demo.o(i.pps_update_handle) for pps_update_handle
    p6a_demo.o(i.app_mipi_tx_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) for hal_dsi_tx_ctrl_create_handle
    p6a_demo.o(i.app_mipi_tx_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    p6a_demo.o(i.app_mipi_tx_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) for hal_dsi_tx_ctrl_set_overwrite_rgb
    p6a_demo.o(i.app_mipi_tx_init) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.app_mipi_tx_init) refers to p6a_demo.o(.data) for g_tx_ctrl_handle
    p6a_demo.o(i.app_mipi_tx_start) refers to p6a_demo.o(i.app_init_panel) for app_init_panel
    p6a_demo.o(i.app_mipi_tx_start) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    p6a_demo.o(i.app_mipi_tx_start) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode) for hal_dsi_tx_ctrl_set_tear_mode
    p6a_demo.o(i.app_mipi_tx_start) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) for hal_dsi_rx_ctrl_pre_init_pps
    p6a_demo.o(i.app_mipi_tx_start) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) for hal_dsi_rx_ctrl_toggle_resolution
    p6a_demo.o(i.app_mipi_tx_start) refers to tau_delay.o(i.delayMs) for delayMs
    p6a_demo.o(i.app_mipi_tx_start) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    p6a_demo.o(i.app_mipi_tx_start) refers to hal_swire.o(i.hal_swire_set_pulse) for hal_swire_set_pulse
    p6a_demo.o(i.app_mipi_tx_start) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.app_mipi_tx_start) refers to p6a_demo.o(.data) for g_tx_ctrl_handle
    p6a_demo.o(i.app_system_process) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.app_system_process) refers to p6a_demo.o(i.app_system_suspend) for app_system_suspend
    p6a_demo.o(i.app_system_process) refers to p6a_demo.o(i.app_system_resume) for app_system_resume
    p6a_demo.o(i.app_system_process) refers to p6a_demo.o(.data) for sg_system_suspend
    p6a_demo.o(i.app_system_resume) refers to hal_pwr.o(i.hal_pwr_exit_sleep_mode) for hal_pwr_exit_sleep_mode
    p6a_demo.o(i.app_system_resume) refers to p6a_demo.o(i.app_display_init) for app_display_init
    p6a_demo.o(i.app_system_resume) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.app_system_suspend) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) for hal_dsi_tx_ctrl_stop
    p6a_demo.o(i.app_system_suspend) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) for hal_dsi_tx_ctrl_deinit
    p6a_demo.o(i.app_system_suspend) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) for hal_dsi_rx_ctrl_stop
    p6a_demo.o(i.app_system_suspend) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) for hal_dsi_rx_ctrl_deinit
    p6a_demo.o(i.app_system_suspend) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    p6a_demo.o(i.app_system_suspend) refers to hal_swire.o(i.hal_swire_deinit) for hal_swire_deinit
    p6a_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_set_sleep_mode_power) for hal_pwr_set_sleep_mode_power
    p6a_demo.o(i.app_system_suspend) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    p6a_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_enter_normal_sleep_mode) for hal_pwr_enter_normal_sleep_mode
    p6a_demo.o(i.app_system_suspend) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) for hal_pwr_set_stop_sleep_wakeup_pin
    p6a_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) for hal_pwr_enter_stop_sleep_mode
    p6a_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode) for hal_pwr_enter_deep_sleep_mode
    p6a_demo.o(i.app_system_suspend) refers to p6a_demo.o(.data) for g_tx_ctrl_handle
    p6a_demo.o(i.app_system_suspend) refers to p6a_demo.o(i.ap_rstn_pull_high_cb) for ap_rstn_pull_high_cb
    p6a_demo.o(i.app_tx_panel_reset) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    p6a_demo.o(i.app_tx_panel_reset) refers to tau_delay.o(i.delayMs) for delayMs
    p6a_demo.o(i.google_p6a_demo) refers to hal_gpio.o(i.hal_gpio_set_high_impedance) for hal_gpio_set_high_impedance
    p6a_demo.o(i.google_p6a_demo) refers to hal_pwr.o(i.hal_pwr_set_main_power) for hal_pwr_set_main_power
    p6a_demo.o(i.google_p6a_demo) refers to p6a_demo.o(i.app_display_init) for app_display_init
    p6a_demo.o(i.google_p6a_demo) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.google_p6a_demo) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) for hal_dsi_rx_ctrl_dcs_async_handler
    p6a_demo.o(i.google_p6a_demo) refers to p6a_demo.o(i.app_system_process) for app_system_process
    p6a_demo.o(i.google_p6a_demo) refers to p6a_demo.o(.data) for g_rx_ctrl_handle
    p6a_demo.o(i.pps_update_handle) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode) for hal_dsi_tx_ctrl_set_tear_mode
    p6a_demo.o(i.pps_update_handle) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) for hal_dsi_rx_ctrl_toggle_resolution
    p6a_demo.o(i.pps_update_handle) refers to p6a_demo.o(.data) for g_rx_ctrl_handle
    p6a_demo.o(i.send_panel_init_code) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) for hal_dsi_tx_ctrl_write_array_cmd
    p6a_demo.o(i.send_panel_init_code) refers to tau_delay.o(i.delayUs) for delayUs
    p6a_demo.o(i.soft_te_timer_cb) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) for hal_dsi_tx_ctrl_gen_a_tear_signal
    p6a_demo.o(i.soft_te_timer_cb) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    p6a_demo.o(i.soft_te_timer_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode) for hal_dsi_tx_ctrl_set_tear_mode
    p6a_demo.o(i.soft_te_timer_init) refers to hal_timer.o(i.hal_timer_init) for hal_timer_init
    p6a_demo.o(i.soft_te_timer_init) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    p6a_demo.o(i.soft_te_timer_init) refers to p6a_demo.o(.data) for g_tx_ctrl_handle
    p6a_demo.o(i.soft_te_timer_init) refers to p6a_demo.o(i.soft_te_timer_cb) for soft_te_timer_cb
    p6a_demo.o(.constdata) refers to p6a_demo.o(i.ap_dcs_set_display_on) for ap_dcs_set_display_on
    p6a_demo.o(.constdata) refers to p6a_demo.o(i.ap_dcs_set_display_off) for ap_dcs_set_display_off
    p6a_demo.o(.constdata) refers to p6a_demo.o(i.ap_dcs_set_backlight) for ap_dcs_set_backlight
    p6a_demo.o(.constdata) refers to p6a_demo.o(i.ap_set_FPS_B1) for ap_set_FPS_B1
    p6a_demo.o(.constdata) refers to p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) for ap_dcs_set_enter_sleep_mode
    p6a_demo.o(.constdata) refers to p6a_demo.o(i.ap_dcs_set_exit_sleep_mode) for ap_dcs_set_exit_sleep_mode
    p6a_demo.o(.constdata) refers to p6a_demo.o(i.ap_dcs_set_frame_change) for ap_dcs_set_frame_change
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_init) for hal_system_init
    board.o(i.board_Init) refers to tau_log.o(i.tau_log_init) for tau_log_init
    startup_armcm0.o(RESET) refers to startup_armcm0.o(STACK) for __initial_sp
    startup_armcm0.o(RESET) refers to startup_armcm0.o(.text) for Reset_Handler
    startup_armcm0.o(RESET) refers to drv_common.o(i.HardFault_Handler) for HardFault_Handler
    startup_armcm0.o(RESET) refers to drv_common.o(i.SysTick_Handler) for SysTick_Handler
    startup_armcm0.o(RESET) refers to drv_vidc.o(i.VIDC_IRQn_Handler) for VIDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to hal_internal_vsync.o(i.LCDC_IRQn_Handler) for LCDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) for MIPI_RX_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler) for MIPI_TX_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_memc.o(i.MEMC_IRQn_Handler) for MEMC_IRQn_Handler
    startup_armcm0.o(RESET) refers to hal_internal_dcs.o(i.VPRE_IRQn_Handler) for VPRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_dma.o(i.DMA_IRQn_Handler) for DMA_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER0_IRQn_Handler) for TIMER0_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER1_IRQn_Handler) for TIMER1_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER2_IRQn_Handler) for TIMER2_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER3_IRQn_Handler) for TIMER3_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_uart.o(i.UART_IRQn_Handler) for UART_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_rxbr.o(i.VPRE1_IRQn_Handler) for VPRE1_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_swire.o(i.SWIRE_IRQn_Handler) for SWIRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.AP_NRESET_IRQn_Handler) for AP_NRESET_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT0_IRQn_Handler) for EXTI_INT0_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT1_IRQn_Handler) for EXTI_INT1_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT2_IRQn_Handler) for EXTI_INT2_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT3_IRQn_Handler) for EXTI_INT3_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT4_IRQn_Handler) for EXTI_INT4_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT5_IRQn_Handler) for EXTI_INT5_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT6_IRQn_Handler) for EXTI_INT6_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT7_IRQn_Handler) for EXTI_INT7_IRQn_Handler
    startup_armcm0.o(.text) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd) refers to drv_rxbr.o(i.drv_rxbr_set_ack_pkt_md) for drv_rxbr_set_ack_pkt_md
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_lpdt_fifo_status) for drv_dsi_rx_get_lpdt_fifo_status
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) for dcs_packet_get_fifo_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) for dcs_packet_free_fifo_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) for hal_internal_vsync_get_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_reset_modules) for drv_crgu_reset_modules
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_rxbr.o(i.drv_rxbr_swpxl_clr) for drv_rxbr_swpxl_clr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_rxbr.o(i.drv_rxbr_set_cmd_filter) for drv_rxbr_set_cmd_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_vidc.o(i.drv_vidc_set_src_parameter) for drv_vidc_set_src_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_vidc.o(i.drv_vidc_set_pu_ctrl) for drv_vidc_set_pu_ctrl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_rxbr.o(i.drv_rxbr_set_swpxl_data) for drv_rxbr_set_swpxl_data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg) for drv_dsi_rx_set_ddi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) for hal_dsi_rx_ctrl_set_rx_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg) for drv_dsi_rx_set_ipi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.constdata) for .constdata
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_force_video_crtl) refers to drv_dsi_rx.o(i.drv_dsi_rx_force_video_crtl) for drv_dsi_rx_force_video_crtl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size) for drv_dsi_rx_get_max_ret_size
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) for hal_dsi_rx_ctrl_init_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_rx) for hal_internal_vsync_init_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) for hal_dsi_rx_ctrl_init_dsi_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) for hal_dsi_rx_ctrl_init_rxbr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_irqen) for drv_dsc_dec_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) for hal_dsi_rx_ctrl_init_vidc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) for hal_dsi_rx_ctrl_init_memc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_se.o(i.drv_se_start_rx) for drv_se_start_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_pwr.o(i.drv_pwr_set_pll_clk) for drv_pwr_set_pll_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_clk) for drv_crgu_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dsc_clk) for drv_crgu_set_dsc_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_vidc_clk) for drv_crgu_set_vidc_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_fb_clk) for drv_crgu_set_fb_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg) for drv_dsi_rx_set_ctrl_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) for drv_dsi_rx_set_up_phy
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap) for drv_dsi_rx_set_lane_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_crc_en) for drv_dsi_rx_set_ddi_crc_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_ycbcr_frmt) for drv_dsi_rx_set_ipi_ycbcr_frmt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_tear_resp_en) for drv_dsi_rx_set_tear_resp_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_inten) for drv_dsi_rx_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc) for drv_dsi_rx_set_check_crc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt) for drv_dsi_rx_set_resp_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_mode) for drv_memc_set_ltpo_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_fs_en_conditions) for drv_memc_set_fs_en_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_lcdc_st_conditions) for drv_memc_set_lcdc_st_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_vidc_sync_cnt) for drv_memc_set_vidc_sync_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_double_buffer) for drv_memc_set_double_buffer
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_circ_mode_enable) for drv_memc_set_circ_mode_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_active_height) for drv_memc_set_active_height
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_pu_thres) for drv_memc_set_ltpo_pu_thres
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_color_format) for drv_rxbr_set_color_format
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th) for drv_rxbr_set_ltpo_drop_th
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_cfg) for drv_rxbr_set_usr_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_col) for drv_rxbr_set_usr_col
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_row) for drv_rxbr_set_usr_row
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg) for drv_rxbr_hline_rcv_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) for hal_intl_dcs_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_src_parameter) for drv_vidc_set_src_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pentile_swap) for drv_vidc_set_pentile_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_dst_parameter) for drv_vidc_set_dst_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_circ_mode_enable) for drv_vidc_set_circ_mode_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_init_module_enable) for drv_vidc_init_module_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_dither_config) for drv_vidc_set_dither_config
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_vintp_config) for drv_vidc_set_vintp_config
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_rotation) for drv_vidc_set_rotation
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef0) for drv_vidc_set_scld_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef1) for drv_vidc_set_scld_hcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef0) for drv_vidc_set_scld_vcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef1) for drv_vidc_set_scld_vcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_honly_hinitr) for drv_vidc_set_honly_hinitr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_honly_hinitb) for drv_vidc_set_honly_hinitb
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_honly_hcoef0) for drv_vidc_set_honly_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_mirror) for drv_vidc_set_mirror
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pu_ctrl) for drv_vidc_set_pu_ctrl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_dsi_rx_ctrl.o(.constdata) for .constdata
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to hal_internal_vsync.o(i.hal_internal_sync_register_rx_callback) for hal_internal_sync_register_rx_callback
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to drv_vidc.o(i.drv_vidc_set_irq_line) for drv_vidc_set_irq_line
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_write_cmd_entry) refers to hal_internal_dcs.o(i.hal_intl_dcs_register_write_cmd_entry) for hal_intl_dcs_register_write_cmd_entry
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header) for drv_rxbr_set_ack_pkt_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack) refers to drv_rxbr.o(i.drv_rxbr_set_cmd_response) for drv_rxbr_set_cmd_response
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) for hal_intl_dcs_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_check_crc) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc) for drv_dsi_rx_set_check_crc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_check_crc) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) for drv_dsi_rx_calc_ipi_tx_delay
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg) for drv_dsi_rx_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_log_level) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_drv_log_level) for drv_dsi_rx_set_drv_log_level
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to drv_rxbr.o(i.drv_rxbr_sw_reset) for drv_rxbr_sw_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) for hal_dsi_rx_ctrl_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) for hal_intl_svs_update_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_clk) for drv_crgu_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_dsi_rx.o(i.drv_dsi_rx_power_up) for drv_dsi_rx_power_up
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) for hal_internal_vsync_toggle_input_frame_rate
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) for hal_internal_sync_input_resolution_change
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) for hal_dsi_tx_ctrl_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg) for drv_dsi_tx_phy_time_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) for drv_dsi_tx_phy_test_setup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready) for drv_dsi_tx_phy_status_ready
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_crgu.o(i.drv_crgu_reset_modules) for drv_crgu_reset_modules
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_reset_modules) for drv_crgu_reset_modules
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb) for hal_internal_sync_register_lcdc_cb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) for hal_internal_sync_set_fb_setting_manual
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) for hal_lcdc_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_frame) refers to drv_lcdc.o(i.drv_lcdc_fixed_frame_output) for drv_lcdc_fixed_frame_output
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_get_tear_mode) for drv_memc_get_tear_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_gen_a_tear_signal) for drv_memc_gen_a_tear_signal
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_tx) for hal_internal_vsync_init_tx
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb) for hal_internal_sync_register_lcdc_cb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) for hal_dsi_tx_ctrl_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) for hal_dsi_tx_init_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) for hal_dsi_tx_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) for hal_lcdc_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) for hal_lcdc_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready) for drv_dsi_tx_phy_status_ready
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) for hal_nonshadow_func_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_vsync_func_update) for hal_vsync_func_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_overwrite_enable) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_overwrite_enable) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_partial_disp_enable) refers to drv_lcdc.o(i.drv_lcdc_part_display_config) for drv_lcdc_part_display_config
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_partial_disp_enable) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload) for drv_dsi_tx_command_get_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) for hal_nonshadow_func_req_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_sync_line) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) for hal_internal_vsync_set_sync_line
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_sync_line) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) for hal_nonshadow_func_req_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) for hal_nonshadow_func_req_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) for hal_nonshadow_func_req_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb) for drv_lcdc_config_overwrite_rgb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_vpg) for drv_dsi_tx_set_vpg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) for hal_dsi_tx_ctrl_draw_flick
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_cfg_int_frame) for drv_lcdc_cfg_int_frame
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_enable_shadow_reg) for drv_lcdc_enable_shadow_reg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_start) for hal_lcdc_start
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_lcdc.o(i.drv_lcdc_stop_display) for drv_lcdc_stop_display
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) for hal_dsi_tx_ctrl_read_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg) for drv_dsi_tx_video_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack) for drv_dsi_tx_set_bta_ack
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time) for drv_dsi_tx_dpi_lpcmd_time
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode) for drv_dsi_tx_phy_lane_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode) for drv_dsi_tx_dpi_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity) for drv_dsi_tx_dpi_polarity
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_response_mode) for drv_dsi_tx_response_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div) for drv_dsi_tx_set_time_out_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg) for drv_dsi_tx_timeout_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp) for drv_dsi_tx_phy_clock_lane_auto_lp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_int) for drv_dsi_tx_config_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to drv_crgu.o(i.drv_crgu_set_dpi_clk) for drv_crgu_set_dpi_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to hal_dsi_tx_ctrl.o(.constdata) for .constdata
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg) for drv_dsi_tx_phy_time_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) for drv_dsi_tx_phy_test_setup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update) for hal_dsi_tx_timing_info_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) for hal_dsi_tx_cmd_mode_cal_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size) for drv_dsi_tx_edpi_cmd_size
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) for hal_dsi_tx_init_phy_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) for hal_dsi_tx_init_dpi_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) for hal_dsi_tx_vid_mode_cal_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing) for hal_dsi_tx_init_vid_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk) for drv_dsi_tx_set_video_chunk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing) for drv_dsi_tx_set_video_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_header) for drv_dsi_tx_command_header
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update) refers to d2f.o(.text) for __aeabi_d2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_internal_svs.o(i.hal_intl_svs_init_tx) for hal_intl_svs_init_tx
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) for hal_tx_frame_rate_adjust
    hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) refers to drv_lcdc.o(i.drv_lcdc_endianness_config) for drv_lcdc_endianness_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) refers to drv_lcdc.o(i.drv_lcdc_crop_hact) for drv_lcdc_crop_hact
    hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) for hal_lcdc_postproc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) for hal_lcdc_displayproc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) for hal_intl_fb_get_tx_fb_info
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) for hal_lcdc_timinggen_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to drv_lcdc.o(i.drv_lcdc_config_int) for drv_lcdc_config_int
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fscalb.o(.text) for __ARM_scalbnf
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_lcdc_clk) for drv_crgu_set_lcdc_clk
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) for hal_intl_fb_get_tx_fb_info
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) for hal_lcdc_upscaler_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_fldc_config) for drv_lcdc_fldc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_bcsa_config) for drv_lcdc_bcsa_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_fc_config) for drv_lcdc_fc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_edge_dect_config) for drv_lcdc_edge_dect_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_edge_enh_config) for drv_lcdc_edge_enh_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_vintp_mode_config) for drv_lcdc_vintp_mode_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_dith_config) for drv_lcdc_dith_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to drv_lcdc.o(i.drv_lcdc_vid_hw_start) for drv_lcdc_vid_hw_start
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to drv_lcdc.o(i.drv_lcdc_cmd_start) for drv_lcdc_cmd_start
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to drv_lcdc.o(i.drv_lcdc_ctrl_flow) for drv_lcdc_ctrl_flow
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to drv_lcdc.o(i.drv_lcdc_config_src_parameter) for drv_lcdc_config_src_parameter
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to drv_lcdc.o(i.drv_lcdc_set_prefetch) for drv_lcdc_set_prefetch
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for sg_pq_para
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_bcsa_config) for drv_lcdc_bcsa_config
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_fc_config) for drv_lcdc_fc_config
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_edge_dect_config) for drv_lcdc_edge_dect_config
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_edge_enh_config) for drv_lcdc_edge_enh_config
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for sg_pq_para
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to cfcmple.o(.text) for __aeabi_cfcmple
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_vsync_func_update) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_vsync_func_update) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_gpio.o(i.hal_gpio_config_pad) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_config_pad) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    hal_gpio.o(i.hal_gpio_config_pad) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    hal_gpio.o(i.hal_gpio_ctrl_eint) refers to drv_gpio.o(i.drv_gpio_set_int) for drv_gpio_set_int
    hal_gpio.o(i.hal_gpio_get_input_data) refers to drv_gpio.o(i.drv_gpio_get_input_data) for drv_gpio_get_input_data
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_eint) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group) for drv_sys_cfg_sel_gpio_group
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig) for drv_sys_cfg_sel_int_trig
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_init_input) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_input) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_init_output) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_reg_eint_cb) refers to drv_gpio.o(i.drv_gpio_register_callback) for drv_gpio_register_callback
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_gpio.o(i.drv_gpio_register_ap_reset_callback) for drv_gpio_register_ap_reset_callback
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) for drv_sys_cfg_sel_ap_rst_trig
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_high_impedance) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode) for drv_gpio_set_mode
    hal_gpio.o(i.hal_gpio_set_output_data) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to hal_gpio.o(.constdata) for .constdata
    hal_swire.o(i.hal_swire_deinit) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    hal_swire.o(i.hal_swire_deinit) refers to drv_swire.o(i.drv_swire_enable) for drv_swire_enable
    hal_swire.o(i.hal_swire_deinit) refers to drv_swire.o(i.drv_swire_register_callback) for drv_swire_register_callback
    hal_swire.o(i.hal_swire_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_swire.o(i.hal_swire_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_swire.o(i.hal_swire_deinit) refers to hal_timer.o(i.hal_timer_deinit) for hal_timer_deinit
    hal_swire.o(i.hal_swire_deinit) refers to hal_swire.o(.data) for .data
    hal_swire.o(i.hal_swire_enable) refers to drv_swire.o(i.drv_swire_set_power_down) for drv_swire_set_power_down
    hal_swire.o(i.hal_swire_enable) refers to drv_swire.o(i.drv_swire_get_pulse_count) for drv_swire_get_pulse_count
    hal_swire.o(i.hal_swire_enable) refers to drv_swire.o(i.drv_swire_set_trig_mode) for drv_swire_set_trig_mode
    hal_swire.o(i.hal_swire_enable) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_swire.o(i.hal_swire_enable) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    hal_swire.o(i.hal_swire_enable) refers to hal_swire.o(.data) for .data
    hal_swire.o(i.hal_swire_init) refers to drv_crgu.o(i.drv_crgu_set_clock_div) for drv_crgu_set_clock_div
    hal_swire.o(i.hal_swire_init) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_swire.o(i.hal_swire_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_swire.o(i.hal_swire_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_swire.o(i.hal_swire_init) refers to drv_swire.o(i.drv_swire_set_bit_time) for drv_swire_set_bit_time
    hal_swire.o(i.hal_swire_init) refers to drv_swire.o(i.drv_swire_set_power_down) for drv_swire_set_power_down
    hal_swire.o(i.hal_swire_init) refers to drv_swire.o(i.drv_swire_enable) for drv_swire_enable
    hal_swire.o(i.hal_swire_init) refers to drv_common.o(.data) for g_system_clock
    hal_swire.o(i.hal_swire_register_callback) refers to drv_swire.o(i.drv_swire_register_callback) for drv_swire_register_callback
    hal_swire.o(i.hal_swire_register_callback) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    hal_swire.o(i.hal_swire_set_pulse) refers to drv_swire.o(i.drv_swire_set_trig_mode) for drv_swire_set_trig_mode
    hal_swire.o(i.hal_swire_set_pulse) refers to drv_swire.o(i.drv_swire_set_pulse_count) for drv_swire_set_pulse_count
    hal_swire.o(i.hal_swire_set_pulse) refers to hal_swire.o(.data) for .data
    hal_swire.o(i.hal_swire_set_timer) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_swire_timer) for drv_sys_cfg_sel_swire_timer
    hal_swire.o(i.hal_swire_set_timer) refers to hal_timer.o(i.hal_timer_init) for hal_timer_init
    hal_swire.o(i.hal_swire_set_timer) refers to hal_timer.o(i.hal_timer_set_repeat) for hal_timer_set_repeat
    hal_swire.o(i.hal_swire_set_timer) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_swire.o(i.hal_swire_set_timer) refers to drv_swire.o(i.drv_swire_set_trig_mode) for drv_swire_set_trig_mode
    hal_swire.o(i.hal_swire_set_timer) refers to hal_swire.o(.data) for .data
    hal_swire.o(i.hal_swire_set_waveform) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_swire.o(i.hal_swire_set_waveform) refers to drv_swire.o(i.drv_swire_set_bit_time) for drv_swire_set_bit_time
    hal_swire.o(i.hal_swire_set_waveform) refers to drv_common.o(.data) for g_system_clock
    hal_system.o(i.hal_system_disable_systick) refers to drv_common.o(i.drv_common_disable_systick) for drv_common_disable_systick
    hal_system.o(i.hal_system_enable_systick) refers to drv_common.o(i.drv_common_enable_systick) for drv_common_enable_systick
    hal_system.o(i.hal_system_get_tick) refers to drv_common.o(i.drv_common_get_tick) for drv_common_get_tick
    hal_system.o(i.hal_system_idle_mode) refers to drv_common.o(i.drv_common_idle_mode) for drv_common_idle_mode
    hal_system.o(i.hal_system_init) refers to drv_pwr.o(i.drv_pwr_set_pll_clk) for drv_pwr_set_pll_clk
    hal_system.o(i.hal_system_init) refers to hal_system.o(i.hal_system_updata_sysclk) for hal_system_updata_sysclk
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_system.o(i.hal_system_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int) for drv_sys_cfg_clear_all_int
    hal_system.o(i.hal_system_init) refers to drv_common.o(i.drv_common_system_init) for drv_common_system_init
    hal_system.o(i.hal_system_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_system.o(i.hal_system_register_systick_cb) refers to drv_common.o(i.drv_common_systick_register_cb) for drv_common_systick_register_cb
    hal_system.o(i.hal_system_reset_chip) refers to drv_crgu.o(i.drv_crgu_reset_chip) for drv_crgu_reset_chip
    hal_system.o(i.hal_system_updata_sysclk) refers to drv_crgu.o(i.drv_crgu_set_ahb_clk) for drv_crgu_set_ahb_clk
    hal_system.o(i.hal_system_updata_sysclk) refers to drv_common.o(.data) for g_system_clock
    hal_system.o(i.hal_system_updata_sysclk) refers to drv_common.o(.data) for g_system_delay_step
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_set_repeat) for drv_timer_set_repeat
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_timer.o(i.hal_timer_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_timer.o(i.hal_timer_get_status) refers to drv_timer.o(i.drv_timer_get_status) for drv_timer_get_status
    hal_timer.o(i.hal_timer_init) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_timer.o(i.hal_timer_init) refers to drv_timer.o(i.drv_timer_set_prescaler) for drv_timer_set_prescaler
    hal_timer.o(i.hal_timer_set_repeat) refers to drv_timer.o(i.drv_timer_set_repeat) for drv_timer_set_repeat
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_pwr.o(i.hal_pwr_elvcc_close) refers to drv_pwr.o(i.drv_pwr_pwmled_electric_current) for drv_pwr_pwmled_electric_current
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_pwmled_electric_current) for drv_pwr_pwmled_electric_current
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_hv_ldo_mode_sel) for drv_pwr_hv_ldo_mode_sel
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_hv_ldo_mode_clock_sel) for drv_pwr_hv_ldo_mode_clock_sel
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_pwmled_driver_current_Big_step) for drv_pwr_pwmled_driver_current_Big_step
    hal_pwr.o(i.hal_pwr_elvcc_vol_set) refers to drv_pwr.o(i.drv_pwr_hv_ldo_voltage_set) for drv_pwr_hv_ldo_voltage_set
    hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode) refers to drv_pwr.o(i.drv_pwr_set_wakeup_type) for drv_pwr_set_wakeup_type
    hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode) for drv_pwr_enter_deep_sleep_mode
    hal_pwr.o(i.hal_pwr_enter_normal_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_sleep_mode_ex) for drv_pwr_enter_sleep_mode_ex
    hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_stop_sleep_mode) for drv_pwr_enter_stop_sleep_mode
    hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) refers to hal_pwr.o(.data) for .data
    hal_pwr.o(i.hal_pwr_exit_sleep_mode) refers to drv_pwr.o(i.drv_pwr_exit_sleep_mode) for drv_pwr_exit_sleep_mode
    hal_pwr.o(i.hal_pwr_get_reset_flag) refers to drv_crgu.o(i.drv_crgu_get_all_reset_flag) for drv_crgu_get_all_reset_flag
    hal_pwr.o(i.hal_pwr_get_reset_flag) refers to drv_pwr.o(i.drv_pwr_get_wakeflag) for drv_pwr_get_wakeflag
    hal_pwr.o(i.hal_pwr_get_reset_flag) refers to drv_crgu.o(i.drv_crgu_clear_all_reset_flags) for drv_crgu_clear_all_reset_flags
    hal_pwr.o(i.hal_pwr_get_vcc_power_ready) refers to drv_pwr.o(i.drv_pwr_get_power_ready_st) for drv_pwr_get_power_ready_st
    hal_pwr.o(i.hal_pwr_ldo13s_en) refers to drv_pwr.o(i.drv_pwr_ldo13s_en) for drv_pwr_ldo13s_en
    hal_pwr.o(i.hal_pwr_ldo13s_set) refers to drv_pwr.o(i.drv_pwr_ldo13s_set) for drv_pwr_ldo13s_set
    hal_pwr.o(i.hal_pwr_ldo18s_en) refers to drv_pwr.o(i.drv_pwr_ldo18s_en) for drv_pwr_ldo18s_en
    hal_pwr.o(i.hal_pwr_ldo18s_set) refers to drv_pwr.o(i.drv_pwr_ldo18s_set) for drv_pwr_ldo18s_set
    hal_pwr.o(i.hal_pwr_set_main_power) refers to drv_pwr.o(i.drv_pwr_set_digit_power_sel) for drv_pwr_set_digit_power_sel
    hal_pwr.o(i.hal_pwr_set_pvd) refers to drv_pwr.o(i.drv_pwr_set_pvd) for drv_pwr_set_pvd
    hal_pwr.o(i.hal_pwr_set_sleep_mode_power) refers to drv_pwr.o(i.drv_pwr_set_breath_screen_power_sel) for drv_pwr_set_breath_screen_power_sel
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_ctrl_eint) for hal_gpio_ctrl_eint
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_init_eint) for hal_gpio_init_eint
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_reg_eint_cb) for hal_gpio_reg_eint_cb
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_pwr.o(.data) for .data
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_pwr.o(i.stop_sleep_cb) for stop_sleep_cb
    hal_pwr.o(i.hal_pwr_set_vcc_enable) refers to drv_pwr.o(i.drv_pwr_charge_pump_en) for drv_pwr_charge_pump_en
    hal_pwr.o(i.stop_sleep_cb) refers to hal_pwr.o(.data) for .data
    tau_delay.o(i.delayMs) refers to tau_delay.o(i.delayUs) for delayUs
    tau_delay.o(i.delayUs) refers to drv_common.o(.data) for g_system_delay_step
    tau_log.o(i.fgetc) refers to hal_uart.o(i.hal_uart_recv_blocking) for hal_uart_recv_blocking
    tau_log.o(i.fgetc) refers to hal_system.o(i.hal_system_get_debug_state) for hal_system_get_debug_state
    tau_log.o(i.fgetc) refers to hal_system.o(i.hal_system_clear_debug_state) for hal_system_clear_debug_state
    tau_log.o(i.fgetc) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.fputc) refers to tau_log.o(i.tau_log_push_log) for tau_log_push_log
    tau_log.o(i.fputc) refers to hal_uart.o(i.hal_uart_send_blocking) for hal_uart_send_blocking
    tau_log.o(i.fputc) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.tau_log_init) refers to hal_uart.o(i.hal_uart_init) for hal_uart_init
    tau_log.o(i.tau_log_init) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.tau_log_printf) refers to memseta.o(.text) for __aeabi_memclr4
    tau_log.o(i.tau_log_printf) refers to strlen.o(.text) for strlen
    tau_log.o(i.tau_log_printf) refers to printfa.o(i.__0vsprintf) for vsprintf
    tau_log.o(i.tau_log_printf) refers to tau_log.o(i.tau_log_push_log) for tau_log_push_log
    tau_log.o(i.tau_log_printf) refers to printfa.o(i.__0printf) for __2printf
    tau_log.o(i.tau_log_printf) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.tau_log_printf) refers to tau_log.o(.bss) for g_log_buf
    tau_log.o(i.tau_log_push_log) refers to memcpya.o(.text) for __aeabi_memcpy
    tau_log.o(i.tau_log_push_log) refers to tau_delay.o(i.delayUs) for delayUs
    tau_log.o(.ARM.__at_0x1101C) refers to tau_log.o(.bss) for g_log_buf
    hal_uart.o(i.hal_uart0_rx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart0_tx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart1_rx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart1_tx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_deinit) refers to drv_uart.o(i.drv_uart_deinit) for drv_uart_deinit
    hal_uart.o(i.hal_uart_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_uart.o(i.hal_uart_deinit) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_dma_path_close) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_uart.o(i.hal_uart_dma_path_close) refers to drv_dma.o(i.drv_dma_deinit) for drv_dma_deinit
    hal_uart.o(i.hal_uart_dma_path_close) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_apply_handle) for drv_dma_apply_handle
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_set_burst) for drv_dma_set_burst
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_register_callback) for drv_dma_register_callback
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_enable_int) for drv_dma_enable_int
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_set_mem_trans_info) for drv_dma_set_mem_trans_info
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_enable) for drv_dma_enable
    hal_uart.o(i.hal_uart_dma_recv) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_uart.o(i.hal_uart_dma_recv) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_dma_recv) refers to hal_uart.o(i.hal_uart0_rx_dma_cb) for hal_uart0_rx_dma_cb
    hal_uart.o(i.hal_uart_dma_recv) refers to hal_uart.o(i.hal_uart1_rx_dma_cb) for hal_uart1_rx_dma_cb
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_apply_handle) for drv_dma_apply_handle
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_set_burst) for drv_dma_set_burst
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_register_callback) for drv_dma_register_callback
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_enable_int) for drv_dma_enable_int
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_set_mem_trans_info) for drv_dma_set_mem_trans_info
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_enable) for drv_dma_enable
    hal_uart.o(i.hal_uart_dma_send) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_uart.o(i.hal_uart_dma_send) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_dma_send) refers to hal_uart.o(i.hal_uart0_tx_dma_cb) for hal_uart0_tx_dma_cb
    hal_uart.o(i.hal_uart_dma_send) refers to hal_uart.o(i.hal_uart1_tx_dma_cb) for hal_uart1_tx_dma_cb
    hal_uart.o(i.hal_uart_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_uart.o(i.hal_uart_init) refers to drv_uart.o(i.drv_uart_init) for drv_uart_init
    hal_uart.o(i.hal_uart_init) refers to drv_uart.o(i.drv_uart_trans_create_handle) for drv_uart_trans_create_handle
    hal_uart.o(i.hal_uart_init) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_init) refers to drv_common.o(.data) for g_system_clock
    hal_uart.o(i.hal_uart_init) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_recv_blocking) refers to drv_uart.o(i.drv_uart_recv_blocking) for drv_uart_recv_blocking
    hal_uart.o(i.hal_uart_recv_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_recv_none_blocking) refers to drv_uart.o(i.drv_uart_recv_none_blocking) for drv_uart_recv_none_blocking
    hal_uart.o(i.hal_uart_recv_none_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_send_blocking) refers to drv_uart.o(i.drv_uart_send_blocking) for drv_uart_send_blocking
    hal_uart.o(i.hal_uart_send_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_send_none_blocking) refers to drv_uart.o(i.drv_uart_send_none_blocking) for drv_uart_send_none_blocking
    hal_uart.o(i.hal_uart_send_none_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_internal_vsync.o(i.LCDC_IRQn_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.LCDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_internal_vsync.o(i.LCDC_IRQn_Handler) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) for hal_intl_fb_cal_fb_info
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) for hal_dsi_tx_ctrl_gen_a_tear_signal
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_delay.o(i.delayUs) for delayUs
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) for hal_vsync_reset_lcdc_scaler
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_sync_register_rx_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) for hal_intl_fb_set_fb_info_manual
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) for hal_intl_fb_cal_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_svs.o(i.hal_intl_svs_init_rx) for hal_intl_svs_init_rx
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr) for hal_intl_dcs_init_sw_fltr
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_rxbr.o(i.drv_rxbr_register_irq1_callback) for drv_rxbr_register_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_vidc.o(i.drv_vidc_register_callback) for drv_vidc_register_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_init) for dcs_packet_fifo_init
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_gen_te) for soft_gen_te
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_gen_te_double_buffer) for soft_gen_te_double_buffer
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.rxbr_irq1_callback) for rxbr_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.vidc_callback) for vidc_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) for hal_intl_fb_cal_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_svs.o(i.hal_intl_svs_deinit_rx) for hal_intl_svs_deinit_rx
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_svs.o(i.hal_intl_svs_set_sync_coef) for hal_intl_svs_set_sync_coef
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_memc.o(i.drv_memc_set_frame_drop_select) for drv_memc_set_frame_drop_select
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_set_tear_line) for drv_lcdc_set_tear_line
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_config_acc_command_mode) for drv_lcdc_config_acc_command_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_svs.o(i.hal_intl_svs_deinit_tx) for hal_intl_svs_deinit_tx
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_svs.o(i.hal_intl_svs_set_input_frate) for hal_intl_svs_set_input_frate
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg) for drv_rxbr_hline_rcv0_cfg
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dadd.o(.text) for __aeabi_dadd
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_int_source) for drv_rxbr_get_int_source
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.soft_double_buffer_update) for soft_double_buffer_update
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_svs.o(i.hal_intl_svs_handle) for hal_intl_svs_handle
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.vpre_err_reset) for vpre_err_reset
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_lcdc.o(i.drv_lcdc_cmd_start) for drv_lcdc_cmd_start
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt) for hal_intl_svs_set_rx_vtt
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.soft_double_buffer_update) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.soft_gen_te_double_buffer) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_gen_te_double_buffer) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_get_int_source) for drv_vidc_get_int_source
    hal_internal_vsync.o(i.vidc_callback) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_clear_irq) for drv_vidc_clear_irq
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_get_irq_status) for drv_vidc_get_irq_status
    hal_internal_vsync.o(i.vidc_callback) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.vpre_err_reset) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to hal_internal_dcs.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) for hal_intl_dcs_rx_receive_packet
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_dsc_dec.o(i.drv_dsc_dec_get_nslc) for drv_dsc_dec_get_nslc
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_crgu.o(i.drv_crgu_set_dsc_clk) for drv_crgu_set_dsc_clk
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to hal_internal_dcs.o(.data) for .data
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to hal_internal_dcs.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr) refers to hal_internal_dcs.o(.bss) for .bss
    hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_register_write_cmd_entry) refers to hal_internal_dcs.o(.data) for .data
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle) for hal_intl_dcs_sw_filter_handle
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) for dcs_packet_fifo_alloc
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) for hal_dsi_rx_ctrl_dcs_async_handler
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_ddi_crc_en) for drv_dsi_rx_get_ddi_crc_en
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_dcs.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_dcs.o(.data) for .data
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_dcs.o(.conststring) for .conststring
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) for hal_intl_dcs_rx_get_dcs_packet_data
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) for hal_intl_dcs_rx_receive_pps
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to hal_internal_dcs.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to hal_internal_dcs.o(.conststring) for .conststring
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) refers to memseta.o(.text) for __aeabi_memset
    hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) refers to drv_rxbr.o(i.drv_rxbr_set_filter_regs) for drv_rxbr_set_filter_regs
    hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) refers to hal_internal_dcs.o(.bss) for .bss
    hal_internal_dcs.o(i.hal_intl_dcs_set_dcs_direct_mode) refers to hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) for hal_intl_dcs_set_auto_hw_filter
    hal_internal_dcs.o(i.hal_intl_dcs_set_dcs_direct_mode) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle) refers to hal_internal_dcs.o(.data) for .data
    hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle) refers to hal_internal_dcs.o(.bss) for .bss
    hal_internal_dcs.o(.data) refers to hal_internal_dcs.o(.bss) for g_imm_buffer
    hal_internal_fb.o(i.ha_intl_fb_check_pu_size) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.ha_intl_fb_check_pu_size) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter) for hal_intl_fb_flow_control_adapter
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) for hal_intl_fb_check_bandwidth
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.ha_intl_fb_check_pu_size) for ha_intl_fb_check_pu_size
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.hal_intl_fb_edge_resize) for hal_intl_fb_edge_resize
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_fb.o(i.hal_intl_fb_edge_resize) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.hal_intl_fb_edge_resize) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_user_flow) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to hal_internal_fb.o(.conststring) for .conststring
    hal_internal_svs.o(i.hal_intl_svs_deinit_rx) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.hal_intl_svs_deinit_rx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_deinit_rx) refers to hal_internal_svs.o(i.svs_wait_start) for svs_wait_start
    hal_internal_svs.o(i.hal_intl_svs_deinit_tx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_handle) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) for hal_intl_svs_update_rxbr_clk
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_svs.o(i.svs_wait_start) for svs_wait_start
    hal_internal_svs.o(i.hal_intl_svs_init_tx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_svs.o(i.svs_wait_start) for svs_wait_start
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_svs.o(i.svs_wait_fr_stab) for svs_wait_fr_stab
    hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_set_sync_coef) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to dmul.o(.text) for __aeabi_dmul
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg) for drv_rxbr_hline_rcv1_cfg
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_get_rel_intv) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_svs.o(i.svs_get_rel_intv) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_sync_handle) refers to hal_internal_svs.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_svs.o(i.svs_sync_handle) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_svs.o(i.svs_sync_handle) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_svs.o(i.svs_sync_handle) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_svs.o(i.svs_sync_handle) refers to f2d.o(.text) for __aeabi_f2d
    hal_internal_svs.o(i.svs_sync_handle) refers to dadd.o(.text) for __aeabi_dadd
    hal_internal_svs.o(i.svs_sync_handle) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_svs.o(i.svs_sync_handle) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to hal_internal_svs.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to ffixui.o(.text) for __aeabi_f2uiz
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to hal_internal_svs.o(i.svs_sync_handle) for svs_sync_handle
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_svs.o(i.svs_wait_start) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_internal_svs.o(i.svs_wait_start) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_svs.o(i.svs_wait_start) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_internal_svs.o(i.svs_wait_start) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_svs.o(i.svs_wait_start) refers to f2d.o(.text) for __aeabi_f2d
    hal_internal_svs.o(i.svs_wait_start) refers to ceil.o(i.ceil) for ceil
    hal_internal_svs.o(i.svs_wait_start) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(i.svs_direct_mode_setting) for svs_direct_mode_setting
    hal_internal_svs.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_svs.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg) for drv_rxbr_hline_rcv1_cfg
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(i.svs_wait_fr_stab) for svs_wait_fr_stab
    drv_common.o(i.HardFault_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_common.o(i.SysTick_Handler) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_enable_systick) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_common.o(i.drv_common_enable_systick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_get_tick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_system_init) refers to drv_se.o(i.drv_se_init) for drv_se_init
    drv_common.o(i.drv_common_systick_register_cb) refers to drv_common.o(.data) for .data
    drv_crgu.o(i.drv_crgu_get_rxbr_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_crgu.o(i.drv_crgu_get_system_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to drv_se.o(i.drv_se_set_dsc) for drv_se_set_dsc
    drv_gpio.o(i.AP_NRESET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.AP_NRESET_IRQn_Handler) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.EXTI_INT0_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT1_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT2_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT3_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT4_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT5_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT6_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT7_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.drv_gpio_handle_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.drv_gpio_handle_int) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_register_ap_reset_callback) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.drv_gpio_register_callback) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_pwr.o(i.drv_pwr_analog_pwm_en) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_elvcc_pwm_en) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_elvcc_pwm_en) refers to tau_delay.o(i.delayMs) for delayMs
    drv_pwr.o(i.drv_pwr_enter_sleep_mode) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_enter_sleep_mode) refers to drv_pwr.o(i.drv_pwr_por_mode_flag) for drv_pwr_por_mode_flag
    drv_pwr.o(i.drv_pwr_enter_stop_sleep_mode) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_exit_sleep_mode) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_hv_ldo_mode_clock_sel) refers to drv_pwr.o(i.drv_pwr_hv_ldo_10M_clock) for drv_pwr_hv_ldo_10M_clock
    drv_pwr.o(i.drv_pwr_pwm_output_pwm_led) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_breath_screen_power_sel) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_digit_power_sel) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_system_clk) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_wakeup_type) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_swire.o(i.SWIRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_swire.o(i.SWIRE_IRQn_Handler) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_register_callback) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_sys_cfg.o(i.drv_sys_cfg_sel_dma_req) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_timer.o(i.TIMER0_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.TIMER1_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.TIMER2_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.TIMER3_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_timer.o(i.drv_timer_enable) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_get_instance) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_get_status) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_clear_status_flags) for drv_timer_clear_status_flags
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_register_callback) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_compare_val) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_compare_val) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_timer.o(i.drv_timer_set_compare_val) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_compare_val) refers to drv_common.o(.data) for g_system_clock
    drv_timer.o(i.drv_timer_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_repeat) refers to drv_timer.o(.data) for .data
    dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_fifo_init) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_size) refers to dcs_packet_fifo.o(.bss) for .bss
    drv_se.o(i.drv_se_init) refers to drv_efuse.o(i.drv_efuse_enter_inactive) for drv_efuse_enter_inactive
    drv_se.o(i.drv_se_init) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_se.o(i.drv_se_init) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_dsc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_dsc) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_lcdc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_lcdc) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_memc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_memc) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_rxbr) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_rxbr) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_vidc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_vidc) refers to drv_se.o(.data) for .data
    drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) refers to drv_dsi_rx.o(.data) for .data
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) for drv_dsi_rx_get_color_bpp
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to ffltui.o(.text) for __aeabi_ui2f
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fdiv.o(.text) for __aeabi_fdiv
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fmul.o(.text) for __aeabi_fmul
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc) for drv_dsi_rx_get_color_pcc
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fadd.o(.text) for __aeabi_fadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to cfrcmple.o(.text) for __aeabi_cfrcmple
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to f2d.o(.text) for __aeabi_f2d
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dadd.o(.text) for __aeabi_dadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dfixui.o(.text) for __aeabi_d2uiz
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_set_drv_log_level) refers to drv_dsi_rx.o(.data) for .data
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_test_lock) for drv_phy_test_lock
    drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_enter) for drv_tx_phy_test_enter
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_code) for drv_tx_phy_test_write_code
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_exit) for drv_tx_phy_test_exit
    drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_version) for drv_dsi_tx_version
    drv_dsi_tx.o(i.drv_dsi_tx_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_tx.o(i.drv_dsi_tx_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_lcdc.o(i.drv_lcdc_clear_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_lcdc.o(i.drv_lcdc_cmd_start) refers to drv_se.o(i.drv_se_set_lcdc) for drv_se_set_lcdc
    drv_lcdc.o(i.drv_lcdc_ctrl_flow) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    drv_lcdc.o(i.drv_lcdc_part_display_config) refers to drv_lcdc.o(i.drv_lcdc_pixel_value_config) for drv_lcdc_pixel_value_config
    drv_lcdc.o(i.drv_lcdc_set_int) refers to drv_lcdc.o(i.drv_lcdc_clear_int) for drv_lcdc_clear_int
    drv_lcdc.o(i.drv_lcdc_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_lcdc.o(i.drv_lcdc_vid_hw_start) refers to drv_se.o(i.drv_se_set_lcdc) for drv_se_set_lcdc
    drv_memc.o(i.MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_get_status) for drv_memc_get_status
    drv_memc.o(i.MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_clear_status) for drv_memc_clear_status
    drv_memc.o(i.MEMC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_memc.o(i.drv_memc_rate_transfer_sel) refers to drv_se.o(i.drv_se_set_memc) for drv_se_set_memc
    drv_memc.o(i.drv_memc_set_ltpo_mode) refers to drv_se.o(i.drv_se_set_memc) for drv_se_set_memc
    drv_rxbr.o(i.VPRE1_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.VPRE1_IRQn_Handler) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_EnableIRQ) for __NVIC_EnableIRQ
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_rxbr.o(i.drv_rxbr_register_irq0_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_register_irq1_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_set_cmd_filter) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_rxbr.o(i.drv_rxbr_set_cmd_response) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_rxbr.o(i.drv_rxbr_set_color_format) refers to drv_se.o(i.drv_se_set_rxbr) for drv_se_set_rxbr
    drv_rxbr.o(i.drv_rxbr_soft_reset) refers to tau_delay.o(i.delayMs) for delayMs
    drv_rxbr.o(i.drv_rxbr_sw_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_rxbr.o(i.drv_rxbr_sw_reset) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    drv_vidc.o(i.VIDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.VIDC_IRQn_Handler) refers to drv_vidc.o(.data) for .data
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_vidc.o(i.drv_vidc_register_callback) refers to drv_vidc.o(.data) for .data
    drv_vidc.o(i.drv_vidc_set_src_parameter) refers to drv_se.o(i.drv_se_set_vidc) for drv_se_set_vidc
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(i.drv_dma_get_int_source) for drv_dma_get_int_source
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(i.drv_dma_clear_status) for drv_dma_clear_status
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(.data) for .data
    drv_dma.o(i.drv_dma_apply_handle) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dma.o(i.drv_dma_apply_handle) refers to drv_dma.o(.data) for .data
    drv_dma.o(i.drv_dma_apply_handle) refers to drv_dma.o(.constdata) for .constdata
    drv_dma.o(i.drv_dma_deinit) refers to drv_dma.o(i.drv_dma_disable_int) for drv_dma_disable_int
    drv_dma.o(i.drv_dma_disable_int) refers to drv_dma.o(i.drv_dma_int_list_delete) for drv_dma_int_list_delete
    drv_dma.o(i.drv_dma_disable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.drv_dma_enable_int) refers to drv_dma.o(i.drv_dma_int_list_inset) for drv_dma_int_list_inset
    drv_dma.o(i.drv_dma_enable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dma.o(i.drv_dma_init) refers to drv_per_common.o(i.drv_per_set_clock) for drv_per_set_clock
    drv_dma.o(i.drv_dma_init) refers to drv_dma.o(i.drv_dma_update_handle_setting) for drv_dma_update_handle_setting
    drv_dma.o(i.drv_dma_int_list_delete) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_int_list_inset) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_update_handle_setting) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_dma_req) for drv_sys_cfg_sel_dma_req
    drv_dma.o(i.drv_dma_update_req_by_default) refers to drv_dma.o(i.drv_dma_update_handle_setting) for drv_dma_update_handle_setting
    drv_dma.o(i.drv_dma_update_req_by_default) refers to drv_dma.o(.constdata) for .constdata
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_int_trans_handle) for drv_uart_int_trans_handle
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_abort_recv) for drv_uart_abort_recv
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_abort_send) for drv_uart_abort_send
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(.constdata) for .constdata
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(i.drv_uart_reset_rx_fifo) for drv_uart_reset_rx_fifo
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(i.drv_uart_reset_tx_fifo) for drv_uart_reset_tx_fifo
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_deinit) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_deinit) refers to drv_uart.o(i.drv_uart_enable_clk) for drv_uart_enable_clk
    drv_uart.o(i.drv_uart_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.drv_uart_deinit) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_enable_clk) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    drv_uart.o(i.drv_uart_enable_int) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_enable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.drv_uart_get_def_cfg) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.drv_uart_get_def_cfg) refers to drv_common.o(.data) for g_system_clock
    drv_uart.o(i.drv_uart_get_instance) refers to drv_uart.o(.constdata) for .constdata
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_enable_clk) for drv_uart_enable_clk
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_set_baud_rate) for drv_uart_set_baud_rate
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_enable_int) for drv_uart_enable_int
    drv_uart.o(i.drv_uart_int_trans_handle) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_recv_none_blocking) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_recv_none_blocking) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_recv_none_blocking) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_reset_rx_fifo) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_reset_tx_fifo) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_send_none_blocking) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_send_none_blocking) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_send_none_blocking) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_set_baud_rate) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_uart.o(i.drv_uart_trans_create_handle) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_trans_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.drv_uart_trans_create_handle) refers to drv_uart.o(.bss) for .bss
    drv_efuse.o(i.drv_efuse_enter_inactive) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    drv_efuse.o(i.drv_efuse_enter_inactive) refers to drv_efuse.o(i.drv_efuse_int_enable) for drv_efuse_int_enable
    drv_efuse.o(i.drv_efuse_read) refers to drv_pwr.o(i.drv_pwr_efuse_pd) for drv_pwr_efuse_pd
    drv_efuse.o(i.drv_efuse_read) refers to drv_efuse.o(i.drv_efuse_read_req) for drv_efuse_read_req
    drv_efuse.o(i.drv_efuse_write) refers to drv_pwr.o(i.drv_pwr_efuse_pd) for drv_pwr_efuse_pd
    drv_efuse.o(i.drv_efuse_write) refers to drv_efuse.o(i.drv_efuse_write_req) for drv_efuse_write_req
    drv_efuse.o(i.drv_efuse_write_read_req_clear) refers to drv_efuse.o(i.drv_efuse_write_req) for drv_efuse_write_req
    drv_efuse.o(i.drv_efuse_write_read_req_clear) refers to drv_efuse.o(i.drv_efuse_read_req) for drv_efuse_read_req
    drv_per_common.o(i.drv_per_get_system_clk) refers to drv_crgu.o(i.drv_crgu_get_system_clk) for drv_crgu_get_system_clk
    drv_per_common.o(i.drv_per_reset_module) refers to drv_crgu.o(i.drv_crgu_reset_modules) for drv_crgu_reset_modules
    drv_per_common.o(i.drv_per_set_clock) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    ceil.o(i.__softfp_ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.__softfp_ceil) refers to ceil.o(i.ceil) for ceil
    ceil.o(i.ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.ceil) refers to dadd.o(.text) for __aeabi_dadd
    ceil.o(i.ceil) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry10a.o(.ARM.Collect$$$$0000000D) for __rt_final_cpp
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry11a.o(.ARM.Collect$$$$0000000F) for __rt_final_exit
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry7b.o(.ARM.Collect$$$$00000008) for _main_clock
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry8b.o(.ARM.Collect$$$$0000000A) for _main_cpp_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry9a.o(.ARM.Collect$$$$0000000B) for _main_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry5.o(.ARM.Collect$$$$00000004) for _main_scatterload
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry2.o(.ARM.Collect$$$$00000001) for _main_stk
    idiv.o(.text) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfb.o(i.__0fprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0fprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0printf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printfb.o(i.__0vfprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vfprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printf0.o(i.__0fprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0fprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0printf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf0.o(i.__0vfprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vfprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf1.o(i.__0fprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0fprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0printf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i.__0vfprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vfprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf2.o(i.__0fprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0fprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0printf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf2.o(i.__0vfprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vfprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf3.o(i.__0fprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0fprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0printf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i.__0vfprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vfprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf4.o(i.__0fprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0fprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0printf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i.__0vfprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vfprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf5.o(i.__0fprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0fprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0printf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i.__0vfprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vfprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf6.o(i.__0fprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0fprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0printf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i.__0vfprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vfprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i._printf_core) refers to printf6.o(i._printf_pre_padding) for _printf_pre_padding
    printf6.o(i._printf_core) refers to printf6.o(i._printf_post_padding) for _printf_post_padding
    printf6.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf7.o(i.__0fprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0fprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0printf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i.__0vfprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vfprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i._printf_core) refers to printf7.o(i._printf_pre_padding) for _printf_pre_padding
    printf7.o(i._printf_core) refers to printf7.o(i._printf_post_padding) for _printf_post_padding
    printf7.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf8.o(i.__0fprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0fprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0printf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i.__0vfprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vfprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i._printf_core) refers to printf8.o(i._printf_pre_padding) for _printf_pre_padding
    printf8.o(i._printf_core) refers to printf8.o(i._printf_post_padding) for _printf_post_padding
    printf8.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i.__0fprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0fprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0fprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0printf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0printf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0snprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0snprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0snprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0sprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0sprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0sprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i.__0vfprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vfprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vfprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0vsnprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0vsprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i._fp_digits) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._fp_digits) refers to dmul.o(.text) for __aeabi_dmul
    printfa.o(i._fp_digits) refers to ddiv.o(.text) for __aeabi_ddiv
    printfa.o(i._fp_digits) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    printfa.o(i._fp_digits) refers to dadd.o(.text) for __aeabi_dadd
    printfa.o(i._fp_digits) refers to dfixul.o(.text) for __aeabi_d2ulz
    printfa.o(i._fp_digits) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_core) refers to printfa.o(i._printf_pre_padding) for _printf_pre_padding
    printfa.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers to printfa.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i._printf_core) refers to printfa.o(i._fp_digits) for _fp_digits
    printfa.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfa.o(i._printf_post_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_pre_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._snputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._sputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    fmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers to fepilogue.o(.text) for _float_round
    fscalb.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    dadd.o(.text) refers to llsshr.o(.text) for __aeabi_lasr
    dadd.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dmul.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ffltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ffltui.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    dfltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfltui.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ffixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixui.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    f2d.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    d2f.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    d2f.o(.text) refers to fepilogue.o(.text) for _float_round
    cfcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    cfrcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    entry2.o(.ARM.Collect$$$$00000001) refers to entry2.o(.ARM.Collect$$$$00002712) for __lit__00000000
    entry2.o(.ARM.Collect$$$$00002712) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    entry5.o(.ARM.Collect$$$$00000004) refers to init.o(.text) for __scatterload
    entry9a.o(.ARM.Collect$$$$0000000B) refers to main.o(i.main) for main
    entry9b.o(.ARM.Collect$$$$0000000C) refers to main.o(i.main) for main
    uldiv.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    uldiv.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to depilogue.o(i.__ARM_clz) for __ARM_clz
    depilogue.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    ddiv.o(.text) refers to depilogue.o(.text) for _double_round
    dfixul.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixul.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    init.o(.text) refers to entry5.o(.ARM.Collect$$$$00000004) for __main_after_scatterload


==============================================================================

Removing Unused input sections from the image.

    Removing main.o(.rev16_text), (4 bytes).
    Removing main.o(.revsh_text), (4 bytes).
    Removing p6a_demo.o(.rev16_text), (4 bytes).
    Removing p6a_demo.o(.revsh_text), (4 bytes).
    Removing p6a_demo.o(i.Gpio_swire_output), (80 bytes).
    Removing p6a_demo.o(i.Panel_CCM), (42 bytes).
    Removing p6a_demo.o(i.REG_51_OFF_output), (60 bytes).
    Removing p6a_demo.o(i.ap_dcs_set_exit_idle_mode), (100 bytes).
    Removing p6a_demo.o(i.soft_te_timer_cb), (28 bytes).
    Removing p6a_demo.o(i.soft_te_timer_init), (40 bytes).
    Removing board.o(.rev16_text), (4 bytes).
    Removing board.o(.revsh_text), (4 bytes).
    Removing startup_armcm0.o(HEAP), (3072 bytes).
    Removing hal_dsi_rx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd), (220 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_short_cmd), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init), (320 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern), (260 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_force_video_crtl), (12 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en), (8 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback), (52 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_write_cmd_entry), (10 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle), (40 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart), (68 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack), (176 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_check_crc), (24 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk), (32 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter), (44 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_log_level), (8 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data), (240 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk), (72 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk), (56 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate), (10 bytes).
    Removing hal_dsi_tx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode), (112 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick), (244 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_frame), (12 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_get_disp_line), (12 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_overwrite_enable), (22 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_partial_disp_enable), (70 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd), (128 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle), (32 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs), (60 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm), (8 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_sync_line), (36 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect), (60 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance), (60 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness), (12 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div), (52 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc), (60 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg), (28 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera), (68 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update), (16 bytes).
    Removing hal_gpio.o(.rev16_text), (4 bytes).
    Removing hal_gpio.o(.revsh_text), (4 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_input_data), (18 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_int_type), (20 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_pull_state), (40 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_driving_strength), (44 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_schmitt_trigger), (52 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_slew_rate), (52 bytes).
    Removing hal_swire.o(.rev16_text), (4 bytes).
    Removing hal_swire.o(.revsh_text), (4 bytes).
    Removing hal_swire.o(i.hal_swire_register_callback), (22 bytes).
    Removing hal_swire.o(i.hal_swire_set_waveform), (92 bytes).
    Removing hal_system.o(.rev16_text), (4 bytes).
    Removing hal_system.o(.revsh_text), (4 bytes).
    Removing hal_system.o(i.hal_system_clear_debug_state), (10 bytes).
    Removing hal_system.o(i.hal_system_disable_systick), (8 bytes).
    Removing hal_system.o(i.hal_system_enable_systick), (8 bytes).
    Removing hal_system.o(i.hal_system_get_debug_state), (8 bytes).
    Removing hal_system.o(i.hal_system_get_tick), (8 bytes).
    Removing hal_system.o(i.hal_system_idle_mode), (8 bytes).
    Removing hal_system.o(i.hal_system_register_systick_cb), (8 bytes).
    Removing hal_system.o(i.hal_system_reset_chip), (10 bytes).
    Removing hal_timer.o(.rev16_text), (4 bytes).
    Removing hal_timer.o(.revsh_text), (4 bytes).
    Removing hal_timer.o(i.hal_timer_get_status), (8 bytes).
    Removing hal_timer.o(i.hal_timer_start), (48 bytes).
    Removing hal_timer.o(i.hal_timer_start_ex), (42 bytes).
    Removing hal_timer.o(i.hal_timer_stop), (40 bytes).
    Removing hal_pwr.o(.rev16_text), (4 bytes).
    Removing hal_pwr.o(.revsh_text), (4 bytes).
    Removing hal_pwr.o(i.hal_pwr_elvcc_close), (10 bytes).
    Removing hal_pwr.o(i.hal_pwr_elvcc_ldo_en), (46 bytes).
    Removing hal_pwr.o(i.hal_pwr_elvcc_vol_set), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_get_reset_flag), (66 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo13s_en), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo13s_set), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo18s_en), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo18s_set), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_set_pvd), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_set_vcc_enable), (8 bytes).
    Removing tau_delay.o(.rev16_text), (4 bytes).
    Removing tau_delay.o(.revsh_text), (4 bytes).
    Removing tau_log.o(.rev16_text), (4 bytes).
    Removing tau_log.o(.revsh_text), (4 bytes).
    Removing tau_log.o(i.fgetc), (72 bytes).
    Removing hal_uart.o(.rev16_text), (4 bytes).
    Removing hal_uart.o(.revsh_text), (4 bytes).
    Removing hal_uart.o(i.hal_uart0_rx_dma_cb), (20 bytes).
    Removing hal_uart.o(i.hal_uart0_tx_dma_cb), (36 bytes).
    Removing hal_uart.o(i.hal_uart1_rx_dma_cb), (20 bytes).
    Removing hal_uart.o(i.hal_uart1_tx_dma_cb), (36 bytes).
    Removing hal_uart.o(i.hal_uart_deinit), (48 bytes).
    Removing hal_uart.o(i.hal_uart_dma_path_close), (92 bytes).
    Removing hal_uart.o(i.hal_uart_dma_recv), (276 bytes).
    Removing hal_uart.o(i.hal_uart_dma_send), (280 bytes).
    Removing hal_uart.o(i.hal_uart_recv_blocking), (28 bytes).
    Removing hal_uart.o(i.hal_uart_recv_none_blocking), (28 bytes).
    Removing hal_uart.o(i.hal_uart_send_none_blocking), (28 bytes).
    Removing hal_internal_vsync.o(.rev16_text), (4 bytes).
    Removing hal_internal_vsync.o(.revsh_text), (4 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te), (2 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_register_rx_callback), (28 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual), (28 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line), (60 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate), (134 bytes).
    Removing hal_internal_vsync.o(.data), (4 bytes).
    Removing hal_internal_dcs.o(.rev16_text), (4 bytes).
    Removing hal_internal_dcs.o(.revsh_text), (4 bytes).
    Removing hal_internal_dcs.o(i.hal_intl_dcs_register_write_cmd_entry), (12 bytes).
    Removing hal_internal_dcs.o(i.hal_intl_dcs_set_dcs_direct_mode), (44 bytes).
    Removing hal_internal_fb.o(.rev16_text), (4 bytes).
    Removing hal_internal_fb.o(.revsh_text), (4 bytes).
    Removing hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual), (480 bytes).
    Removing hal_internal_fb.o(.conststring), (152 bytes).
    Removing hal_internal_svs.o(.rev16_text), (4 bytes).
    Removing hal_internal_svs.o(.revsh_text), (4 bytes).
    Removing hal_internal_svs.o(i.hal_intl_svs_set_input_frate), (112 bytes).
    Removing hal_internal_svs.o(i.hal_intl_svs_set_sync_coef), (12 bytes).
    Removing drv_common.o(.rev16_text), (4 bytes).
    Removing drv_common.o(.revsh_text), (4 bytes).
    Removing drv_common.o(i.drv_common_disable_systick), (20 bytes).
    Removing drv_common.o(i.drv_common_enable_systick), (88 bytes).
    Removing drv_common.o(i.drv_common_get_tick), (12 bytes).
    Removing drv_common.o(i.drv_common_idle_mode), (40 bytes).
    Removing drv_common.o(i.drv_common_systick_register_cb), (12 bytes).
    Removing drv_crgu.o(.rev16_text), (4 bytes).
    Removing drv_crgu.o(.revsh_text), (4 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_all_reset_flags), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_reset_flag), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_all_reset_flag), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_reset_flag), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_system_clk), (104 bytes).
    Removing drv_crgu.o(i.drv_crgu_reset_chip), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_clock_src), (16 bytes).
    Removing drv_dsc_dec.o(.rev16_text), (4 bytes).
    Removing drv_dsc_dec.o(.revsh_text), (4 bytes).
    Removing drv_gpio.o(.rev16_text), (4 bytes).
    Removing drv_gpio.o(.revsh_text), (4 bytes).
    Removing drv_gpio.o(i.drv_gpio_get_input_data), (24 bytes).
    Removing drv_pwr.o(.rev16_text), (4 bytes).
    Removing drv_pwr.o(.revsh_text), (4 bytes).
    Removing drv_pwr.o(i.drv_pwr_10bit_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_analog_pwm_en), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_charge_pump_en), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_close_iov18_tp18), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_dsc_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_elvcc_pwm_en), (124 bytes).
    Removing drv_pwr.o(i.drv_pwr_enter_sleep_mode), (152 bytes).
    Removing drv_pwr.o(i.drv_pwr_exit_sleep_mode_ex), (40 bytes).
    Removing drv_pwr.o(i.drv_pwr_fb_pd), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_get_wakeflag), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_get_write_lock_st), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_hf_frm_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_10M_clock), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_mode_clock_sel), (60 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_mode_sel), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_voltage_set), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo11d_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo13s_en), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo13s_set), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo15_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo18s_en), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo18s_set), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_ltpo_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_osc32k_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_osc80m_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_p3k_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_por_mode_flag), (32 bytes).
    Removing drv_pwr.o(i.drv_pwr_power_in), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_power_ready_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_power_sel), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwm_output_pwm_led), (56 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_driver_current_Big_step), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_driver_current_small_step), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_electric_current), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_open_drain), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_ram_pd_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_read_boot_chipst), (12 bytes).
    Removing drv_pwr.o(i.drv_pwr_read_chipcfg), (12 bytes).
    Removing drv_pwr.o(i.drv_pwr_rgbr_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_ap_rst_mode), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_ldo11_mode), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_ldo15_mode), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_pvd), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_pvd_mode), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_system_clk), (32 bytes).
    Removing drv_pwr.o(i.drv_pwr_sw_tp18_en), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_wakeflag_get), (16 bytes).
    Removing drv_swire.o(.rev16_text), (4 bytes).
    Removing drv_swire.o(.revsh_text), (4 bytes).
    Removing drv_sys_cfg.o(.rev16_text), (4 bytes).
    Removing drv_sys_cfg.o(.revsh_text), (4 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_sel_dma_req), (128 bytes).
    Removing drv_timer.o(.rev16_text), (4 bytes).
    Removing drv_timer.o(.revsh_text), (4 bytes).
    Removing drv_timer.o(i.drv_timer_get_status), (38 bytes).
    Removing drv_timer.o(i.drv_timer_register_callback), (20 bytes).
    Removing dcs_packet_fifo.o(.rev16_text), (4 bytes).
    Removing dcs_packet_fifo.o(.revsh_text), (4 bytes).
    Removing dcs_packet_fifo.o(i.dcs_packet_get_fifo_size), (16 bytes).
    Removing drv_se.o(.rev16_text), (4 bytes).
    Removing drv_se.o(.revsh_text), (4 bytes).
    Removing drv_dsi_rx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_rx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_force_video_crtl), (28 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_lpdt_fifo_status), (16 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate), (68 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_version), (12 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg), (24 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_drv_log_level), (12 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg), (48 bytes).
    Removing drv_dsi_tx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_tx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_force_interrupt), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_get_phy_status), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_forcepll), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_start), (24 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot), (68 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger), (92 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter), (296 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit), (228 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_sdf_3d), (32 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_bta), (28 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_vpg), (100 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_version), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_vid_shadow), (20 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_clear), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_lock), (32 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_read), (16 bytes).
    Removing drv_lcdc.o(.rev16_text), (4 bytes).
    Removing drv_lcdc.o(.revsh_text), (4 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_clear_irq), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_dpisignal_output_ctrl), (44 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_fixed_frame_output), (56 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_dpbuf_num), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_dpi_status), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_frame_clk_count), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_int_en_status), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_int_status), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_line_status), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_rgb2pen_subpixel), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_part_display_config), (52 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_pixel_value_config), (32 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_rd_st_line_config), (28 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_software_reset), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_update_shadow_reg), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_vid_sw_start), (56 bytes).
    Removing drv_memc.o(.rev16_text), (4 bytes).
    Removing drv_memc.o(.revsh_text), (4 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_frm_time), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_int_frame), (36 bytes).
    Removing drv_memc.o(i.drv_memc_set_double_buffer_reverse), (24 bytes).
    Removing drv_memc.o(i.drv_memc_set_fb_pri), (44 bytes).
    Removing drv_memc.o(i.drv_memc_set_fb_remaining_line_trigger), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_inten), (28 bytes).
    Removing drv_memc.o(i.drv_memc_set_read_trigger_line), (24 bytes).
    Removing drv_memc.o(i.drv_memc_set_te_ind), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_tear_hwclr), (24 bytes).
    Removing drv_memc.o(i.drv_memc_set_vidc_fb_arb), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_write_trigger_line), (24 bytes).
    Removing drv_rxbr.o(.rev16_text), (4 bytes).
    Removing drv_rxbr.o(.revsh_text), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_clr_swp_cnt), (16 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_dsc_flush), (24 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_col_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_cur_hline_rcv_cnt), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_frame_data_interval), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_hline_dcat), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_ipi_vsync_interval), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_page_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_pix_fmt), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_swpxl_cnt), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg), (20 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_register_irq0_callback), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_ack_pkt_md), (28 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_cmd_filter), (320 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_cmd_response), (324 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_col_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_compress), (32 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_data_catch_hline), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_page_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_swpxl_data), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_tmpdith_bp), (28 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_soft_reset), (32 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_sw_reset), (164 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_swpxl_clr), (32 bytes).
    Removing drv_vidc.o(.rev16_text), (4 bytes).
    Removing drv_vidc.o(.revsh_text), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_clear_status0), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_cap_pixel), (28 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_signal_frame), (36 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status0), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status1), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status2), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_dsc_thresh), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_frmst_latency), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_inff_thresh), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_irq_line), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_module_enable), (28 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_outff_thresh), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_update_src_format), (20 bytes).
    Removing drv_dma.o(.rev16_text), (4 bytes).
    Removing drv_dma.o(.revsh_text), (4 bytes).
    Removing drv_dma.o(i.drv_dma_apply_handle), (304 bytes).
    Removing drv_dma.o(i.drv_dma_deinit), (52 bytes).
    Removing drv_dma.o(i.drv_dma_disable), (20 bytes).
    Removing drv_dma.o(i.drv_dma_disable_int), (40 bytes).
    Removing drv_dma.o(i.drv_dma_enable), (36 bytes).
    Removing drv_dma.o(i.drv_dma_enable_int), (68 bytes).
    Removing drv_dma.o(i.drv_dma_get_remaining_trans_num), (20 bytes).
    Removing drv_dma.o(i.drv_dma_get_status), (20 bytes).
    Removing drv_dma.o(i.drv_dma_init), (22 bytes).
    Removing drv_dma.o(i.drv_dma_int_list_delete), (88 bytes).
    Removing drv_dma.o(i.drv_dma_int_list_inset), (48 bytes).
    Removing drv_dma.o(i.drv_dma_register_callback), (4 bytes).
    Removing drv_dma.o(i.drv_dma_reset), (36 bytes).
    Removing drv_dma.o(i.drv_dma_set_bitwide), (56 bytes).
    Removing drv_dma.o(i.drv_dma_set_burst), (20 bytes).
    Removing drv_dma.o(i.drv_dma_set_circle_mode), (40 bytes).
    Removing drv_dma.o(i.drv_dma_set_dir), (40 bytes).
    Removing drv_dma.o(i.drv_dma_set_increment), (72 bytes).
    Removing drv_dma.o(i.drv_dma_set_mem_trans_info), (40 bytes).
    Removing drv_dma.o(i.drv_dma_set_mem_trans_offset), (24 bytes).
    Removing drv_dma.o(i.drv_dma_set_per_address), (20 bytes).
    Removing drv_dma.o(i.drv_dma_set_priority), (32 bytes).
    Removing drv_dma.o(i.drv_dma_set_tran_int_cnt), (28 bytes).
    Removing drv_dma.o(i.drv_dma_update_handle_setting), (148 bytes).
    Removing drv_dma.o(i.drv_dma_update_req_by_default), (40 bytes).
    Removing drv_dma.o(.constdata), (136 bytes).
    Removing drv_uart.o(.rev16_text), (4 bytes).
    Removing drv_uart.o(.revsh_text), (4 bytes).
    Removing drv_uart.o(i.drv_uart_deinit), (60 bytes).
    Removing drv_uart.o(i.drv_uart_get_def_cfg), (72 bytes).
    Removing drv_uart.o(i.drv_uart_recv_blocking), (48 bytes).
    Removing drv_uart.o(i.drv_uart_recv_none_blocking), (60 bytes).
    Removing drv_uart.o(i.drv_uart_send_none_blocking), (60 bytes).
    Removing drv_efuse.o(.rev16_text), (4 bytes).
    Removing drv_efuse.o(.revsh_text), (4 bytes).
    Removing drv_efuse.o(i.drv_efuse_crc_cal), (128 bytes).
    Removing drv_efuse.o(i.drv_efuse_get_default_config), (26 bytes).
    Removing drv_efuse.o(i.drv_efuse_int_disable), (12 bytes).
    Removing drv_efuse.o(i.drv_efuse_write), (56 bytes).
    Removing drv_efuse.o(i.drv_efuse_write_read_req_clear), (22 bytes).
    Removing drv_efuse.o(i.drv_efuse_write_req), (22 bytes).
    Removing drv_phy_common.o(.rev16_text), (4 bytes).
    Removing drv_phy_common.o(.revsh_text), (4 bytes).
    Removing drv_per_common.o(.rev16_text), (4 bytes).
    Removing drv_per_common.o(.revsh_text), (4 bytes).
    Removing drv_per_common.o(i.drv_per_get_system_clk), (8 bytes).
    Removing drv_per_common.o(i.drv_per_reset_module), (14 bytes).
    Removing drv_per_common.o(i.drv_per_set_clock), (14 bytes).

369 unused section(s) (total 17292 bytes) removed from the image.

==============================================================================

Image Symbol Table

    Local Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    ../clib/../cmprslib/zerorunl2.c          0x00000000   Number         0  __dczerorl2.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uldiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  idiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uidiv.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry5.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry2.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8a.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llshl.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llushr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llsshr.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf7.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfb.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf2.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf0.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf8.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf6.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfa.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf5.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf1.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf4.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf3.o ABSOLUTE
    ../clib/microlib/printf/stubs.s          0x00000000   Number         0  stubs.o ABSOLUTE
    ../clib/microlib/stdio/streams.c         0x00000000   Number         0  stdout.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpya.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpyb.o ABSOLUTE
    ../clib/microlib/string/memset.c         0x00000000   Number         0  memseta.o ABSOLUTE
    ../clib/microlib/string/strlen.c         0x00000000   Number         0  strlen.o ABSOLUTE
    ../clib/microlib/stubs.s                 0x00000000   Number         0  iusefp.o ABSOLUTE
    ../fplib/microlib/d2f.c                  0x00000000   Number         0  d2f.o ABSOLUTE
    ../fplib/microlib/f2d.c                  0x00000000   Number         0  f2d.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  dadd.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  fadd.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  ddiv.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  fdiv.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  depilogue.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  fepilogue.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  ffixui.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixui.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixul.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  ffltui.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  dfltui.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  dmul.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  fmul.o ABSOLUTE
    ../fplib/microlib/fpscalb.c              0x00000000   Number         0  fscalb.o ABSOLUTE
    ../mathlib/ceil.c                        0x00000000   Number         0  ceil.o ABSOLUTE
    ..\..\..\src\common\tau_delay.c          0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\..\..\src\common\tau_log.c            0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_per_common.c 0x00000000   Number         0  drv_per_common.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_pwr.c 0x00000000   Number         0  hal_pwr.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_swire.c 0x00000000   Number         0  hal_swire.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_timer.c 0x00000000   Number         0  hal_timer.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\dcs_packet_fifo.c 0x00000000   Number         0  dcs_packet_fifo.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_dcs.c 0x00000000   Number         0  hal_internal_dcs.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_fb.c 0x00000000   Number         0  hal_internal_fb.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_svs.c 0x00000000   Number         0  hal_internal_svs.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\src\drv_se.c  0x00000000   Number         0  drv_se.o ABSOLUTE
    ..\..\src\app\P6A\p6a_demo.c             0x00000000   Number         0  p6a_demo.o ABSOLUTE
    ..\..\src\app\main.c                     0x00000000   Number         0  main.o ABSOLUTE
    ..\..\src\board\board.c                  0x00000000   Number         0  board.o ABSOLUTE
    ..\..\src\board\startup\startup_ARMCM0.s 0x00000000   Number         0  startup_armcm0.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_delay.c     0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_log.c       0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_per_common.c 0x00000000   Number         0  drv_per_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_pwr.c 0x00000000   Number         0  hal_pwr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_swire.c 0x00000000   Number         0  hal_swire.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_timer.c 0x00000000   Number         0  hal_timer.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\dcs_packet_fifo.c 0x00000000   Number         0  dcs_packet_fifo.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_dcs.c 0x00000000   Number         0  hal_internal_dcs.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_fb.c 0x00000000   Number         0  hal_internal_fb.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_svs.c 0x00000000   Number         0  hal_internal_svs.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\src\\drv_se.c 0x00000000   Number         0  drv_se.o ABSOLUTE
    ..\\..\\src\\app\\P6A\\p6a_demo.c        0x00000000   Number         0  p6a_demo.o ABSOLUTE
    ..\\..\\src\\app\\main.c                 0x00000000   Number         0  main.o ABSOLUTE
    ..\\..\\src\\board\\board.c              0x00000000   Number         0  board.o ABSOLUTE
    cdrcmple.s                               0x00000000   Number         0  cdrcmple.o ABSOLUTE
    cfcmple.s                                0x00000000   Number         0  cfcmple.o ABSOLUTE
    cfrcmple.s                               0x00000000   Number         0  cfrcmple.o ABSOLUTE
    dc.s                                     0x00000000   Number         0  dc.o ABSOLUTE
    handlers.s                               0x00000000   Number         0  handlers.o ABSOLUTE
    init.s                                   0x00000000   Number         0  init.o ABSOLUTE
    RESET                                    0x00010000   Section      192  startup_armcm0.o(RESET)
    .ARM.Collect$$$$00000000                 0x000100c0   Section        0  entry.o(.ARM.Collect$$$$00000000)
    .ARM.Collect$$$$00000001                 0x000100c0   Section        4  entry2.o(.ARM.Collect$$$$00000001)
    .ARM.Collect$$$$00000004                 0x000100c4   Section        4  entry5.o(.ARM.Collect$$$$00000004)
    .ARM.Collect$$$$00000008                 0x000100c8   Section        0  entry7b.o(.ARM.Collect$$$$00000008)
    .ARM.Collect$$$$0000000A                 0x000100c8   Section        0  entry8b.o(.ARM.Collect$$$$0000000A)
    .ARM.Collect$$$$0000000B                 0x000100c8   Section        8  entry9a.o(.ARM.Collect$$$$0000000B)
    .ARM.Collect$$$$0000000D                 0x000100d0   Section        0  entry10a.o(.ARM.Collect$$$$0000000D)
    .ARM.Collect$$$$0000000F                 0x000100d0   Section        0  entry11a.o(.ARM.Collect$$$$0000000F)
    .ARM.Collect$$$$00002712                 0x000100d0   Section        4  entry2.o(.ARM.Collect$$$$00002712)
    __lit__00000000                          0x000100d0   Data           4  entry2.o(.ARM.Collect$$$$00002712)
    .text                                    0x000100d4   Section      120  startup_armcm0.o(.text)
    .text                                    0x0001014c   Section        0  uidiv.o(.text)
    .text                                    0x00010178   Section        0  idiv.o(.text)
    .text                                    0x000101a0   Section        0  memcpya.o(.text)
    .text                                    0x000101c4   Section        0  memseta.o(.text)
    .text                                    0x000101e8   Section        0  strlen.o(.text)
    .text                                    0x000101f6   Section        0  fadd.o(.text)
    .text                                    0x000102a8   Section        0  fmul.o(.text)
    .text                                    0x00010322   Section        0  fdiv.o(.text)
    .text                                    0x0001039e   Section        0  fscalb.o(.text)
    .text                                    0x000103b8   Section        0  dadd.o(.text)
    .text                                    0x0001051c   Section        0  dmul.o(.text)
    .text                                    0x000105ec   Section        0  ffltui.o(.text)
    .text                                    0x000105fc   Section        0  dfltui.o(.text)
    .text                                    0x00010618   Section        0  ffixui.o(.text)
    .text                                    0x00010640   Section        0  dfixui.o(.text)
    .text                                    0x0001067c   Section        0  f2d.o(.text)
    .text                                    0x000106a4   Section        0  d2f.o(.text)
    .text                                    0x000106dc   Section       20  cfcmple.o(.text)
    .text                                    0x000106f0   Section       20  cfrcmple.o(.text)
    .text                                    0x00010704   Section        0  uldiv.o(.text)
    .text                                    0x00010764   Section        0  llshl.o(.text)
    .text                                    0x00010784   Section        0  llushr.o(.text)
    .text                                    0x000107a6   Section        0  llsshr.o(.text)
    .text                                    0x000107cc   Section        0  fepilogue.o(.text)
    .text                                    0x000107cc   Section        0  iusefp.o(.text)
    .text                                    0x0001084e   Section        0  depilogue.o(.text)
    .text                                    0x0001090c   Section        0  ddiv.o(.text)
    .text                                    0x000109fc   Section        0  dfixul.o(.text)
    .text                                    0x00010a3c   Section       40  cdrcmple.o(.text)
    .text                                    0x00010a64   Section       36  init.o(.text)
    .text                                    0x00010a88   Section        0  __dczerorl2.o(.text)
    i.AP_NRESET_IRQn_Handler                 0x00010ae0   Section        0  drv_gpio.o(i.AP_NRESET_IRQn_Handler)
    i.DMA_IRQn_Handler                       0x00010afc   Section        0  drv_dma.o(i.DMA_IRQn_Handler)
    i.EXTI_INT0_IRQn_Handler                 0x00010b58   Section        0  drv_gpio.o(i.EXTI_INT0_IRQn_Handler)
    i.EXTI_INT1_IRQn_Handler                 0x00010b62   Section        0  drv_gpio.o(i.EXTI_INT1_IRQn_Handler)
    i.EXTI_INT2_IRQn_Handler                 0x00010b6c   Section        0  drv_gpio.o(i.EXTI_INT2_IRQn_Handler)
    i.EXTI_INT3_IRQn_Handler                 0x00010b76   Section        0  drv_gpio.o(i.EXTI_INT3_IRQn_Handler)
    i.EXTI_INT4_IRQn_Handler                 0x00010b80   Section        0  drv_gpio.o(i.EXTI_INT4_IRQn_Handler)
    i.EXTI_INT5_IRQn_Handler                 0x00010b8a   Section        0  drv_gpio.o(i.EXTI_INT5_IRQn_Handler)
    i.EXTI_INT6_IRQn_Handler                 0x00010b94   Section        0  drv_gpio.o(i.EXTI_INT6_IRQn_Handler)
    i.EXTI_INT7_IRQn_Handler                 0x00010b9e   Section        0  drv_gpio.o(i.EXTI_INT7_IRQn_Handler)
    i.HardFault_Handler                      0x00010ba8   Section        0  drv_common.o(i.HardFault_Handler)
    i.LCDC_IRQn_Handler                      0x00010bf0   Section        0  hal_internal_vsync.o(i.LCDC_IRQn_Handler)
    i.MEMC_IRQn_Handler                      0x00010cf0   Section        0  drv_memc.o(i.MEMC_IRQn_Handler)
    i.MIPI_TX_IRQn_Handler                   0x00010d8c   Section        0  drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler)
    i.SWIRE_IRQn_Handler                     0x00010e44   Section        0  drv_swire.o(i.SWIRE_IRQn_Handler)
    i.SysTick_Handler                        0x00010e74   Section        0  drv_common.o(i.SysTick_Handler)
    i.TIMER0_IRQn_Handler                    0x00010e8c   Section        0  drv_timer.o(i.TIMER0_IRQn_Handler)
    i.TIMER1_IRQn_Handler                    0x00010e96   Section        0  drv_timer.o(i.TIMER1_IRQn_Handler)
    i.TIMER2_IRQn_Handler                    0x00010ea0   Section        0  drv_timer.o(i.TIMER2_IRQn_Handler)
    i.TIMER3_IRQn_Handler                    0x00010eaa   Section        0  drv_timer.o(i.TIMER3_IRQn_Handler)
    i.VIDC_IRQn_Handler                      0x00010eb4   Section        0  drv_vidc.o(i.VIDC_IRQn_Handler)
    i.VPRE1_IRQn_Handler                     0x00010ed0   Section        0  drv_rxbr.o(i.VPRE1_IRQn_Handler)
    i.VPRE_IRQn_Handler                      0x00010eec   Section        0  hal_internal_dcs.o(i.VPRE_IRQn_Handler)
    i.__0printf                              0x00010f68   Section        0  printfa.o(i.__0printf)
    i.__0vsprintf                            0x00010f88   Section        0  printfa.o(i.__0vsprintf)
    i.__ARM_clz                              0x00010fac   Section        0  depilogue.o(i.__ARM_clz)
    i.__ARM_common_switch8                   0x00010fda   Section        0  hal_dsi_rx_ctrl.o(i.__ARM_common_switch8)
    i.__scatterload_null                     0x00010ff4   Section        2  handlers.o(i.__scatterload_null)
    i._sputc                                 0x00010ff6   Section        0  printfa.o(i._sputc)
    _sputc                                   0x00010ff7   Thumb Code    10  printfa.o(i._sputc)
    .ARM.__at_0x11000                        0x00011000   Section       28  drv_common.o(.ARM.__at_0x11000)
    .ARM.__at_0x1101C                        0x0001101c   Section       16  tau_log.o(.ARM.__at_0x1101C)
    .ARM.__at_0x1102C                        0x0001102c   Section       22  hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C)
    i.MIPI_RX_IRQn_Handler                   0x00011044   Section        0  drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler)
    i.UART_IRQn_Handler                      0x000113a8   Section        0  drv_uart.o(i.UART_IRQn_Handler)
    i.__NVIC_DisableIRQ                      0x00011528   Section        0  drv_rxbr.o(i.__NVIC_DisableIRQ)
    __NVIC_DisableIRQ                        0x00011529   Thumb Code    26  drv_rxbr.o(i.__NVIC_DisableIRQ)
    i.__NVIC_EnableIRQ                       0x00011548   Section        0  drv_rxbr.o(i.__NVIC_EnableIRQ)
    __NVIC_EnableIRQ                         0x00011549   Thumb Code    18  drv_rxbr.o(i.__NVIC_EnableIRQ)
    i.__scatterload_copy                     0x00011560   Section       14  handlers.o(i.__scatterload_copy)
    i.__scatterload_zeroinit                 0x0001156e   Section       14  handlers.o(i.__scatterload_zeroinit)
    i._fp_digits                             0x0001157c   Section        0  printfa.o(i._fp_digits)
    _fp_digits                               0x0001157d   Thumb Code   344  printfa.o(i._fp_digits)
    i._printf_core                           0x000116f0   Section        0  printfa.o(i._printf_core)
    _printf_core                             0x000116f1   Thumb Code  1754  printfa.o(i._printf_core)
    i._printf_post_padding                   0x00011ddc   Section        0  printfa.o(i._printf_post_padding)
    _printf_post_padding                     0x00011ddd   Thumb Code    32  printfa.o(i._printf_post_padding)
    i._printf_pre_padding                    0x00011dfc   Section        0  printfa.o(i._printf_pre_padding)
    _printf_pre_padding                      0x00011dfd   Thumb Code    44  printfa.o(i._printf_pre_padding)
    i.ap_dcs_read                            0x00011e28   Section        0  p6a_demo.o(i.ap_dcs_read)
    ap_dcs_read                              0x00011e29   Thumb Code   280  p6a_demo.o(i.ap_dcs_read)
    i.ap_dcs_set_backlight                   0x00011f6c   Section        0  p6a_demo.o(i.ap_dcs_set_backlight)
    ap_dcs_set_backlight                     0x00011f6d   Thumb Code   146  p6a_demo.o(i.ap_dcs_set_backlight)
    i.ap_dcs_set_display_off                 0x00012010   Section        0  p6a_demo.o(i.ap_dcs_set_display_off)
    ap_dcs_set_display_off                   0x00012011   Thumb Code    50  p6a_demo.o(i.ap_dcs_set_display_off)
    i.ap_dcs_set_display_on                  0x00012068   Section        0  p6a_demo.o(i.ap_dcs_set_display_on)
    ap_dcs_set_display_on                    0x00012069   Thumb Code    90  p6a_demo.o(i.ap_dcs_set_display_on)
    i.ap_dcs_set_enter_sleep_mode            0x00012108   Section        0  p6a_demo.o(i.ap_dcs_set_enter_sleep_mode)
    ap_dcs_set_enter_sleep_mode              0x00012109   Thumb Code    92  p6a_demo.o(i.ap_dcs_set_enter_sleep_mode)
    i.ap_dcs_set_exit_sleep_mode             0x00012190   Section        0  p6a_demo.o(i.ap_dcs_set_exit_sleep_mode)
    ap_dcs_set_exit_sleep_mode               0x00012191   Thumb Code    28  p6a_demo.o(i.ap_dcs_set_exit_sleep_mode)
    i.ap_dcs_set_frame_change                0x000121d0   Section        0  p6a_demo.o(i.ap_dcs_set_frame_change)
    ap_dcs_set_frame_change                  0x000121d1   Thumb Code    46  p6a_demo.o(i.ap_dcs_set_frame_change)
    i.ap_rstn_pull_down_cb                   0x00012204   Section        0  p6a_demo.o(i.ap_rstn_pull_down_cb)
    ap_rstn_pull_down_cb                     0x00012205   Thumb Code    38  p6a_demo.o(i.ap_rstn_pull_down_cb)
    i.ap_rstn_pull_high_cb                   0x0001225c   Section        0  p6a_demo.o(i.ap_rstn_pull_high_cb)
    ap_rstn_pull_high_cb                     0x0001225d   Thumb Code    22  p6a_demo.o(i.ap_rstn_pull_high_cb)
    i.ap_set_FPS_B1                          0x00012278   Section        0  p6a_demo.o(i.ap_set_FPS_B1)
    ap_set_FPS_B1                            0x00012279   Thumb Code    74  p6a_demo.o(i.ap_set_FPS_B1)
    i.app_display_init                       0x000122c2   Section        0  p6a_demo.o(i.app_display_init)
    i.app_gpio_init                          0x000122f0   Section        0  p6a_demo.o(i.app_gpio_init)
    i.app_init_panel                         0x0001230c   Section        0  p6a_demo.o(i.app_init_panel)
    app_init_panel                           0x0001230d   Thumb Code    42  p6a_demo.o(i.app_init_panel)
    i.app_mipi_rx_init                       0x00012340   Section        0  p6a_demo.o(i.app_mipi_rx_init)
    app_mipi_rx_init                         0x00012341   Thumb Code   232  p6a_demo.o(i.app_mipi_rx_init)
    i.app_mipi_tx_init                       0x00012460   Section        0  p6a_demo.o(i.app_mipi_tx_init)
    app_mipi_tx_init                         0x00012461   Thumb Code   216  p6a_demo.o(i.app_mipi_tx_init)
    i.app_mipi_tx_start                      0x0001255c   Section        0  p6a_demo.o(i.app_mipi_tx_start)
    app_mipi_tx_start                        0x0001255d   Thumb Code   120  p6a_demo.o(i.app_mipi_tx_start)
    i.app_system_process                     0x00012604   Section        0  p6a_demo.o(i.app_system_process)
    app_system_process                       0x00012605   Thumb Code    60  p6a_demo.o(i.app_system_process)
    i.app_system_resume                      0x00012670   Section        0  p6a_demo.o(i.app_system_resume)
    app_system_resume                        0x00012671   Thumb Code    30  p6a_demo.o(i.app_system_resume)
    i.app_system_suspend                     0x000126b4   Section        0  p6a_demo.o(i.app_system_suspend)
    app_system_suspend                       0x000126b5   Thumb Code   202  p6a_demo.o(i.app_system_suspend)
    i.app_tx_panel_reset                     0x00012844   Section        0  p6a_demo.o(i.app_tx_panel_reset)
    app_tx_panel_reset                       0x00012845   Thumb Code    46  p6a_demo.o(i.app_tx_panel_reset)
    i.board_Init                             0x00012874   Section        0  board.o(i.board_Init)
    i.ceil                                   0x0001288c   Section        0  ceil.o(i.ceil)
    i.check_mipi_rx_tx_video_info            0x00012954   Section        0  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    check_mipi_rx_tx_video_info              0x00012955   Thumb Code    44  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    i.check_pkt_buf_rev                      0x00012980   Section        0  hal_internal_dcs.o(i.check_pkt_buf_rev)
    check_pkt_buf_rev                        0x00012981   Thumb Code    84  hal_internal_dcs.o(i.check_pkt_buf_rev)
    i.dcs_packet_fifo_alloc                  0x00012a08   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    i.dcs_packet_fifo_init                   0x00012a60   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    i.dcs_packet_free_fifo_header            0x00012a78   Section        0  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    i.dcs_packet_get_fifo_header             0x00012abc   Section        0  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    i.delayMs                                0x00012ae0   Section        0  tau_delay.o(i.delayMs)
    i.delayUs                                0x00012af8   Section        0  tau_delay.o(i.delayUs)
    i.drv_common_system_init                 0x00012b24   Section        0  drv_common.o(i.drv_common_system_init)
    i.drv_crgu_enable_clock                  0x00012b2c   Section        0  drv_crgu.o(i.drv_crgu_enable_clock)
    i.drv_crgu_get_rxbr_clk                  0x00012b68   Section        0  drv_crgu.o(i.drv_crgu_get_rxbr_clk)
    i.drv_crgu_reset_modules                 0x00012bd0   Section        0  drv_crgu.o(i.drv_crgu_reset_modules)
    i.drv_crgu_set_ahb_clk                   0x00012be0   Section        0  drv_crgu.o(i.drv_crgu_set_ahb_clk)
    i.drv_crgu_set_clock_div                 0x00012c08   Section        0  drv_crgu.o(i.drv_crgu_set_clock_div)
    i.drv_crgu_set_dpi_clk                   0x00012c18   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_clk)
    i.drv_crgu_set_dsc_clk                   0x00012c54   Section        0  drv_crgu.o(i.drv_crgu_set_dsc_clk)
    i.drv_crgu_set_fb_clk                    0x00012c8c   Section        0  drv_crgu.o(i.drv_crgu_set_fb_clk)
    i.drv_crgu_set_lcdc_clk                  0x00012cb4   Section        0  drv_crgu.o(i.drv_crgu_set_lcdc_clk)
    i.drv_crgu_set_reset                     0x00012cdc   Section        0  drv_crgu.o(i.drv_crgu_set_reset)
    i.drv_crgu_set_rxbr_clk                  0x00012cf4   Section        0  drv_crgu.o(i.drv_crgu_set_rxbr_clk)
    i.drv_crgu_set_vidc_clk                  0x00012d1c   Section        0  drv_crgu.o(i.drv_crgu_set_vidc_clk)
    i.drv_dma_clear_status                   0x00012d44   Section        0  drv_dma.o(i.drv_dma_clear_status)
    i.drv_dma_get_int_source                 0x00012d5c   Section        0  drv_dma.o(i.drv_dma_get_int_source)
    drv_dma_get_int_source                   0x00012d5d   Thumb Code    16  drv_dma.o(i.drv_dma_get_int_source)
    i.drv_dsc_dec_disable                    0x00012d70   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    i.drv_dsc_dec_enable                     0x00012d8c   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    i.drv_dsc_dec_get_nslc                   0x00012dc4   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    i.drv_dsc_dec_set_irqen                  0x00012de4   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_set_irqen)
    i.drv_dsi_rx_calc_ipi_tx_delay           0x00012e00   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    i.drv_dsi_rx_enable_irq                  0x00012f0c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    i.drv_dsi_rx_get_color_bpp               0x00012f4c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    drv_dsi_rx_get_color_bpp                 0x00012f4d   Thumb Code    62  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    i.drv_dsi_rx_get_color_pcc               0x00012f9c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    drv_dsi_rx_get_color_pcc                 0x00012f9d   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    i.drv_dsi_rx_get_compression_en          0x00012fb8   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    i.drv_dsi_rx_get_ddi_crc_en              0x00012fc8   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_ddi_crc_en)
    i.drv_dsi_rx_get_max_ret_size            0x00012fd8   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size)
    i.drv_dsi_rx_power_up                    0x00012fe4   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    i.drv_dsi_rx_set_check_crc               0x00012ffc   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc)
    i.drv_dsi_rx_set_ctrl_cfg                0x00013018   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    i.drv_dsi_rx_set_ddi_cfg                 0x0001303c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    i.drv_dsi_rx_set_ddi_crc_en              0x0001304c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_crc_en)
    i.drv_dsi_rx_set_inten                   0x00013068   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    i.drv_dsi_rx_set_ipi_cfg                 0x00013074   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    i.drv_dsi_rx_set_ipi_ycbcr_frmt          0x00013084   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_ycbcr_frmt)
    i.drv_dsi_rx_set_lane_swap               0x000130a0   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    i.drv_dsi_rx_set_resp_cnt                0x000130b4   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    i.drv_dsi_rx_set_tear_resp_en            0x000130d8   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_tear_resp_en)
    i.drv_dsi_rx_set_up_phy                  0x000130f4   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    i.drv_dsi_rx_shut_down                   0x000131f4   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    i.drv_dsi_tx_command_header              0x0001320c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    i.drv_dsi_tx_command_mode_cfg            0x00013224   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    i.drv_dsi_tx_command_put_payload         0x0001327c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    i.drv_dsi_tx_config_eotp                 0x00013288   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    i.drv_dsi_tx_config_int                  0x000132a8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    i.drv_dsi_tx_dpi_lpcmd_time              0x000132b4   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    i.drv_dsi_tx_dpi_mode                    0x000132c4   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    i.drv_dsi_tx_dpi_polarity                0x000132d4   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    i.drv_dsi_tx_edpi_cmd_size               0x000132f8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    i.drv_dsi_tx_get_cmd_status              0x00013304   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    i.drv_dsi_tx_mode                        0x00013310   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    i.drv_dsi_tx_phy_clock_lane_auto_lp      0x0001331c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    i.drv_dsi_tx_phy_clock_lane_req_hs       0x00013338   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    i.drv_dsi_tx_phy_lane_mode               0x00013358   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    i.drv_dsi_tx_phy_status_ready            0x00013368   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    i.drv_dsi_tx_phy_status_stopstate        0x000133d0   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    i.drv_dsi_tx_phy_test_setup              0x00013414   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    i.drv_dsi_tx_phy_time_cfg                0x00013564   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    i.drv_dsi_tx_powerup                     0x00013584   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    i.drv_dsi_tx_response_mode               0x00013590   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    i.drv_dsi_tx_set_bta_ack                 0x000135b4   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    i.drv_dsi_tx_set_esc_div                 0x000135d0   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    i.drv_dsi_tx_set_int                     0x000135e4   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    i.drv_dsi_tx_set_time_out_div            0x00013624   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    i.drv_dsi_tx_set_video_chunk             0x0001363c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    i.drv_dsi_tx_set_video_timing            0x00013650   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    i.drv_dsi_tx_shutdown                    0x00013674   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    i.drv_dsi_tx_timeout_cfg                 0x00013680   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    i.drv_dsi_tx_video_mode_cfg              0x000136ac   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    i.drv_efuse_enter_inactive               0x00013794   Section        0  drv_efuse.o(i.drv_efuse_enter_inactive)
    i.drv_efuse_int_enable                   0x000137ca   Section        0  drv_efuse.o(i.drv_efuse_int_enable)
    i.drv_efuse_read                         0x000137d6   Section        0  drv_efuse.o(i.drv_efuse_read)
    i.drv_efuse_read_req                     0x00013810   Section        0  drv_efuse.o(i.drv_efuse_read_req)
    i.drv_gpio_get_attribute                 0x00013828   Section        0  drv_gpio.o(i.drv_gpio_get_attribute)
    i.drv_gpio_handle_int                    0x00013838   Section        0  drv_gpio.o(i.drv_gpio_handle_int)
    drv_gpio_handle_int                      0x00013839   Thumb Code    30  drv_gpio.o(i.drv_gpio_handle_int)
    i.drv_gpio_register_ap_reset_callback    0x0001385c   Section        0  drv_gpio.o(i.drv_gpio_register_ap_reset_callback)
    i.drv_gpio_register_callback             0x00013868   Section        0  drv_gpio.o(i.drv_gpio_register_callback)
    i.drv_gpio_set_attribute                 0x0001387c   Section        0  drv_gpio.o(i.drv_gpio_set_attribute)
    i.drv_gpio_set_int                       0x00013898   Section        0  drv_gpio.o(i.drv_gpio_set_int)
    i.drv_gpio_set_ioe                       0x000138dc   Section        0  drv_gpio.o(i.drv_gpio_set_ioe)
    i.drv_gpio_set_mode                      0x000138fc   Section        0  drv_gpio.o(i.drv_gpio_set_mode)
    i.drv_gpio_set_output_data               0x00013910   Section        0  hal_gpio.o(i.drv_gpio_set_output_data)
    drv_gpio_set_output_data                 0x00013911   Thumb Code    26  hal_gpio.o(i.drv_gpio_set_output_data)
    i.drv_lcdc_bcsa_config                   0x00013930   Section        0  drv_lcdc.o(i.drv_lcdc_bcsa_config)
    i.drv_lcdc_cfg_int_frame                 0x00013958   Section        0  drv_lcdc.o(i.drv_lcdc_cfg_int_frame)
    i.drv_lcdc_clear_int                     0x00013984   Section        0  drv_lcdc.o(i.drv_lcdc_clear_int)
    drv_lcdc_clear_int                       0x00013985   Thumb Code    20  drv_lcdc.o(i.drv_lcdc_clear_int)
    i.drv_lcdc_cmd_start                     0x0001399c   Section        0  drv_lcdc.o(i.drv_lcdc_cmd_start)
    i.drv_lcdc_config_acc_command_mode       0x000139d0   Section        0  drv_lcdc.o(i.drv_lcdc_config_acc_command_mode)
    i.drv_lcdc_config_int                    0x000139e4   Section        0  drv_lcdc.o(i.drv_lcdc_config_int)
    i.drv_lcdc_config_int_single             0x00013a1c   Section        0  drv_lcdc.o(i.drv_lcdc_config_int_single)
    i.drv_lcdc_config_overwrite_rgb          0x00013a44   Section        0  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    i.drv_lcdc_config_src_parameter          0x00013a5c   Section        0  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    i.drv_lcdc_crop_hact                     0x00013aac   Section        0  drv_lcdc.o(i.drv_lcdc_crop_hact)
    i.drv_lcdc_ctrl_flow                     0x00013abc   Section        0  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    i.drv_lcdc_dith_config                   0x00013af4   Section        0  drv_lcdc.o(i.drv_lcdc_dith_config)
    i.drv_lcdc_edge_dect_config              0x00013b24   Section        0  drv_lcdc.o(i.drv_lcdc_edge_dect_config)
    i.drv_lcdc_edge_enh_config               0x00013b60   Section        0  drv_lcdc.o(i.drv_lcdc_edge_enh_config)
    i.drv_lcdc_enable_shadow_reg             0x00013bc4   Section        0  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    i.drv_lcdc_endianness_config             0x00013be8   Section        0  drv_lcdc.o(i.drv_lcdc_endianness_config)
    i.drv_lcdc_fc_config                     0x00013c04   Section        0  drv_lcdc.o(i.drv_lcdc_fc_config)
    i.drv_lcdc_fldc_config                   0x00013c24   Section        0  drv_lcdc.o(i.drv_lcdc_fldc_config)
    i.drv_lcdc_function_disable              0x00013c48   Section        0  drv_lcdc.o(i.drv_lcdc_function_disable)
    i.drv_lcdc_function_enable               0x00013c6c   Section        0  drv_lcdc.o(i.drv_lcdc_function_enable)
    i.drv_lcdc_set_int                       0x00013c90   Section        0  drv_lcdc.o(i.drv_lcdc_set_int)
    i.drv_lcdc_set_prefetch                  0x00013ccc   Section        0  drv_lcdc.o(i.drv_lcdc_set_prefetch)
    i.drv_lcdc_set_tear_line                 0x00013ce8   Section        0  drv_lcdc.o(i.drv_lcdc_set_tear_line)
    i.drv_lcdc_stop_display                  0x00013d04   Section        0  drv_lcdc.o(i.drv_lcdc_stop_display)
    i.drv_lcdc_vid_hw_start                  0x00013d14   Section        0  drv_lcdc.o(i.drv_lcdc_vid_hw_start)
    i.drv_lcdc_vintp_mode_config             0x00013d50   Section        0  drv_lcdc.o(i.drv_lcdc_vintp_mode_config)
    i.drv_memc_clear_status                  0x00013d68   Section        0  drv_memc.o(i.drv_memc_clear_status)
    i.drv_memc_enable_irq                    0x00013d7c   Section        0  drv_memc.o(i.drv_memc_enable_irq)
    i.drv_memc_gen_a_tear_signal             0x00013dbc   Section        0  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    i.drv_memc_get_status                    0x00013dcc   Section        0  drv_memc.o(i.drv_memc_get_status)
    i.drv_memc_get_tear_mode                 0x00013de4   Section        0  drv_memc.o(i.drv_memc_get_tear_mode)
    i.drv_memc_rate_transfer_sel             0x00013df4   Section        0  drv_memc.o(i.drv_memc_rate_transfer_sel)
    i.drv_memc_sel_vsync                     0x00013e10   Section        0  drv_memc.o(i.drv_memc_sel_vsync)
    i.drv_memc_set_active_height             0x00013e24   Section        0  drv_memc.o(i.drv_memc_set_active_height)
    i.drv_memc_set_circ_mode_enable          0x00013e3c   Section        0  drv_memc.o(i.drv_memc_set_circ_mode_enable)
    i.drv_memc_set_data_mode                 0x00013e58   Section        0  drv_memc.o(i.drv_memc_set_data_mode)
    i.drv_memc_set_double_buffer             0x00013e6c   Section        0  drv_memc.o(i.drv_memc_set_double_buffer)
    i.drv_memc_set_frame_drop_select         0x00013e84   Section        0  drv_memc.o(i.drv_memc_set_frame_drop_select)
    i.drv_memc_set_fs_en_conditions          0x00013ea0   Section        0  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    i.drv_memc_set_lcdc_st_conditions        0x00013eb8   Section        0  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    i.drv_memc_set_ltpo_mode                 0x00013ed4   Section        0  drv_memc.o(i.drv_memc_set_ltpo_mode)
    i.drv_memc_set_ltpo_pu_thres             0x00013ef4   Section        0  drv_memc.o(i.drv_memc_set_ltpo_pu_thres)
    i.drv_memc_set_tear_mode                 0x00013f0c   Section        0  drv_memc.o(i.drv_memc_set_tear_mode)
    i.drv_memc_set_tear_waveform             0x00013f20   Section        0  drv_memc.o(i.drv_memc_set_tear_waveform)
    i.drv_memc_set_vidc_sync_cnt             0x00013f4c   Section        0  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    i.drv_phy_test_clear                     0x00013f60   Section        0  drv_phy_common.o(i.drv_phy_test_clear)
    i.drv_phy_test_lock                      0x00013f70   Section        0  drv_phy_common.o(i.drv_phy_test_lock)
    i.drv_pwr_efuse_pd                       0x00013f88   Section        0  drv_pwr.o(i.drv_pwr_efuse_pd)
    i.drv_pwr_enter_deep_sleep_mode          0x00013fb8   Section        0  drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode)
    i.drv_pwr_enter_sleep_mode_ex            0x00014004   Section        0  drv_pwr.o(i.drv_pwr_enter_sleep_mode_ex)
    i.drv_pwr_enter_stop_sleep_mode          0x00014038   Section        0  drv_pwr.o(i.drv_pwr_enter_stop_sleep_mode)
    i.drv_pwr_exit_sleep_mode                0x000140d0   Section        0  drv_pwr.o(i.drv_pwr_exit_sleep_mode)
    i.drv_pwr_get_power_ready_st             0x000140f8   Section        0  drv_pwr.o(i.drv_pwr_get_power_ready_st)
    i.drv_pwr_set_breath_screen_power_sel    0x00014108   Section        0  drv_pwr.o(i.drv_pwr_set_breath_screen_power_sel)
    i.drv_pwr_set_digit_power_sel            0x00014130   Section        0  drv_pwr.o(i.drv_pwr_set_digit_power_sel)
    i.drv_pwr_set_pll_clk                    0x00014158   Section        0  drv_pwr.o(i.drv_pwr_set_pll_clk)
    i.drv_pwr_set_wakeup_type                0x0001418c   Section        0  drv_pwr.o(i.drv_pwr_set_wakeup_type)
    i.drv_pwr_write_lock                     0x000141b8   Section        0  drv_pwr.o(i.drv_pwr_write_lock)
    i.drv_rxbr_clear_pkt_buffer              0x000141d8   Section        0  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    i.drv_rxbr_clear_status0                 0x000141e8   Section        0  drv_rxbr.o(i.drv_rxbr_clear_status0)
    i.drv_rxbr_enable_irq                    0x000141f4   Section        0  drv_rxbr.o(i.drv_rxbr_enable_irq)
    i.drv_rxbr_frame_drop_cfg                0x00014250   Section        0  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    i.drv_rxbr_get_int_source                0x0001426c   Section        0  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    drv_rxbr_get_int_source                  0x0001426d   Thumb Code    20  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    i.drv_rxbr_get_status0                   0x00014284   Section        0  hal_internal_dcs.o(i.drv_rxbr_get_status0)
    drv_rxbr_get_status0                     0x00014285   Thumb Code    20  hal_internal_dcs.o(i.drv_rxbr_get_status0)
    i.drv_rxbr_hline_rcv1_cfg                0x0001429c   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg)
    i.drv_rxbr_hline_rcv_cfg                 0x000142b0   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    i.drv_rxbr_register_irq1_callback        0x000142c0   Section        0  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    i.drv_rxbr_set_ack_pkt_header            0x000142cc   Section        0  drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header)
    i.drv_rxbr_set_color_format              0x000142e4   Section        0  drv_rxbr.o(i.drv_rxbr_set_color_format)
    i.drv_rxbr_set_filter_regs               0x00014300   Section        0  drv_rxbr.o(i.drv_rxbr_set_filter_regs)
    i.drv_rxbr_set_inten                     0x00014324   Section        0  drv_rxbr.o(i.drv_rxbr_set_inten)
    i.drv_rxbr_set_ltpo_drop_th              0x00014340   Section        0  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    i.drv_rxbr_set_usr_cfg                   0x00014358   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    i.drv_rxbr_set_usr_col                   0x00014398   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    i.drv_rxbr_set_usr_row                   0x000143a8   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    i.drv_se_init                            0x000143b8   Section        0  drv_se.o(i.drv_se_init)
    i.drv_se_set_dsc                         0x00014430   Section        0  drv_se.o(i.drv_se_set_dsc)
    i.drv_se_set_lcdc                        0x00014504   Section        0  drv_se.o(i.drv_se_set_lcdc)
    i.drv_se_set_memc                        0x0001458c   Section        0  drv_se.o(i.drv_se_set_memc)
    i.drv_se_set_rxbr                        0x0001461c   Section        0  drv_se.o(i.drv_se_set_rxbr)
    i.drv_se_set_vidc                        0x000146ec   Section        0  drv_se.o(i.drv_se_set_vidc)
    i.drv_se_start_rx                        0x00014798   Section        0  drv_se.o(i.drv_se_start_rx)
    i.drv_swire_enable                       0x000147ac   Section        0  drv_swire.o(i.drv_swire_enable)
    i.drv_swire_get_pulse_count              0x000147c8   Section        0  drv_swire.o(i.drv_swire_get_pulse_count)
    i.drv_swire_register_callback            0x000147d4   Section        0  drv_swire.o(i.drv_swire_register_callback)
    i.drv_swire_set_bit_time                 0x000147e0   Section        0  drv_swire.o(i.drv_swire_set_bit_time)
    i.drv_swire_set_int                      0x000147f8   Section        0  drv_swire.o(i.drv_swire_set_int)
    i.drv_swire_set_power_down               0x00014840   Section        0  drv_swire.o(i.drv_swire_set_power_down)
    i.drv_swire_set_pulse_count              0x0001485c   Section        0  drv_swire.o(i.drv_swire_set_pulse_count)
    i.drv_swire_set_trig_mode                0x00014868   Section        0  drv_swire.o(i.drv_swire_set_trig_mode)
    i.drv_sys_cfg_clear_all_int              0x00014884   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    i.drv_sys_cfg_clear_pending              0x00014890   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    i.drv_sys_cfg_sel_ap_rst_trig            0x000148b8   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig)
    i.drv_sys_cfg_sel_gpio_group             0x000148dc   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group)
    i.drv_sys_cfg_sel_int_trig               0x00014900   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig)
    i.drv_sys_cfg_sel_swire_timer            0x00014924   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_swire_timer)
    i.drv_sys_cfg_set_int                    0x0001493c   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    i.drv_timer_clear_status_flags           0x00014960   Section        0  drv_timer.o(i.drv_timer_clear_status_flags)
    drv_timer_clear_status_flags             0x00014961   Thumb Code    26  drv_timer.o(i.drv_timer_clear_status_flags)
    i.drv_timer_enable                       0x0001497a   Section        0  drv_timer.o(i.drv_timer_enable)
    i.drv_timer_get_instance                 0x0001499c   Section        0  drv_timer.o(i.drv_timer_get_instance)
    i.drv_timer_handle_interrupt             0x000149ac   Section        0  drv_timer.o(i.drv_timer_handle_interrupt)
    drv_timer_handle_interrupt               0x000149ad   Thumb Code    54  drv_timer.o(i.drv_timer_handle_interrupt)
    i.drv_timer_set_compare_val              0x000149e8   Section        0  drv_timer.o(i.drv_timer_set_compare_val)
    i.drv_timer_set_int                      0x00014a28   Section        0  drv_timer.o(i.drv_timer_set_int)
    i.drv_timer_set_prescaler                0x00014a70   Section        0  drv_timer.o(i.drv_timer_set_prescaler)
    i.drv_timer_set_repeat                   0x00014a98   Section        0  drv_timer.o(i.drv_timer_set_repeat)
    i.drv_tx_phy_test_enter                  0x00014aa8   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    i.drv_tx_phy_test_exit                   0x00014ac8   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    i.drv_tx_phy_test_write_code             0x00014ae8   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    i.drv_uart_abort_recv                    0x00014b10   Section        0  drv_uart.o(i.drv_uart_abort_recv)
    i.drv_uart_abort_send                    0x00014b44   Section        0  drv_uart.o(i.drv_uart_abort_send)
    i.drv_uart_config_int                    0x00014b78   Section        0  drv_uart.o(i.drv_uart_config_int)
    i.drv_uart_enable_clk                    0x00014b8c   Section        0  drv_uart.o(i.drv_uart_enable_clk)
    drv_uart_enable_clk                      0x00014b8d   Thumb Code    24  drv_uart.o(i.drv_uart_enable_clk)
    i.drv_uart_enable_int                    0x00014ba4   Section        0  drv_uart.o(i.drv_uart_enable_int)
    i.drv_uart_get_instance                  0x00014c00   Section        0  drv_uart.o(i.drv_uart_get_instance)
    i.drv_uart_init                          0x00014c28   Section        0  drv_uart.o(i.drv_uart_init)
    i.drv_uart_int_trans_handle              0x00014cf8   Section        0  drv_uart.o(i.drv_uart_int_trans_handle)
    drv_uart_int_trans_handle                0x00014cf9   Thumb Code    54  drv_uart.o(i.drv_uart_int_trans_handle)
    i.drv_uart_reset_rx_fifo                 0x00014d34   Section        0  drv_uart.o(i.drv_uart_reset_rx_fifo)
    i.drv_uart_reset_tx_fifo                 0x00014d50   Section        0  drv_uart.o(i.drv_uart_reset_tx_fifo)
    i.drv_uart_send_blocking                 0x00014d6c   Section        0  drv_uart.o(i.drv_uart_send_blocking)
    i.drv_uart_set_baud_rate                 0x00014d86   Section        0  drv_uart.o(i.drv_uart_set_baud_rate)
    i.drv_uart_trans_create_handle           0x00014ddc   Section        0  drv_uart.o(i.drv_uart_trans_create_handle)
    i.drv_vidc_clear_irq                     0x00014e28   Section        0  drv_vidc.o(i.drv_vidc_clear_irq)
    i.drv_vidc_enable                        0x00014e38   Section        0  drv_vidc.o(i.drv_vidc_enable)
    i.drv_vidc_enable_irq                    0x00014e58   Section        0  drv_vidc.o(i.drv_vidc_enable_irq)
    i.drv_vidc_get_int_source                0x00014e98   Section        0  drv_vidc.o(i.drv_vidc_get_int_source)
    i.drv_vidc_get_irq_status                0x00014ec4   Section        0  drv_vidc.o(i.drv_vidc_get_irq_status)
    i.drv_vidc_init_module_enable            0x00014edc   Section        0  drv_vidc.o(i.drv_vidc_init_module_enable)
    i.drv_vidc_register_callback             0x00014f08   Section        0  drv_vidc.o(i.drv_vidc_register_callback)
    i.drv_vidc_reset                         0x00014f14   Section        0  drv_vidc.o(i.drv_vidc_reset)
    i.drv_vidc_set_circ_mode_enable          0x00014f20   Section        0  drv_vidc.o(i.drv_vidc_set_circ_mode_enable)
    i.drv_vidc_set_dither_config             0x00014f3c   Section        0  drv_vidc.o(i.drv_vidc_set_dither_config)
    i.drv_vidc_set_dst_parameter             0x00014f74   Section        0  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    i.drv_vidc_set_honly_hcoef0              0x00014fd0   Section        0  drv_vidc.o(i.drv_vidc_set_honly_hcoef0)
    i.drv_vidc_set_honly_hinitb              0x00014fdc   Section        0  drv_vidc.o(i.drv_vidc_set_honly_hinitb)
    i.drv_vidc_set_honly_hinitr              0x00015008   Section        0  drv_vidc.o(i.drv_vidc_set_honly_hinitr)
    i.drv_vidc_set_irqen                     0x00015038   Section        0  drv_vidc.o(i.drv_vidc_set_irqen)
    i.drv_vidc_set_mirror                    0x00015054   Section        0  drv_vidc.o(i.drv_vidc_set_mirror)
    i.drv_vidc_set_pentile_swap              0x00015068   Section        0  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    i.drv_vidc_set_pu_ctrl                   0x00015084   Section        0  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    i.drv_vidc_set_rotation                  0x00015090   Section        0  drv_vidc.o(i.drv_vidc_set_rotation)
    i.drv_vidc_set_scld_hcoef0               0x000150a8   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    i.drv_vidc_set_scld_hcoef1               0x000150b4   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    i.drv_vidc_set_scld_step                 0x000150c0   Section        0  drv_vidc.o(i.drv_vidc_set_scld_step)
    i.drv_vidc_set_scld_vcoef0               0x000150d4   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    i.drv_vidc_set_scld_vcoef1               0x000150e0   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    i.drv_vidc_set_src_parameter             0x000150ec   Section        0  drv_vidc.o(i.drv_vidc_set_src_parameter)
    i.drv_vidc_set_vintp_config              0x0001510c   Section        0  drv_vidc.o(i.drv_vidc_set_vintp_config)
    i.fputc                                  0x00015144   Section        0  tau_log.o(i.fputc)
    i.google_p6a_demo                        0x00015178   Section        0  p6a_demo.o(i.google_p6a_demo)
    i.ha_intl_fb_check_pu_size               0x000151e0   Section        0  hal_internal_fb.o(i.ha_intl_fb_check_pu_size)
    ha_intl_fb_check_pu_size                 0x000151e1   Thumb Code    58  hal_internal_fb.o(i.ha_intl_fb_check_pu_size)
    i.hal_dsi_rx_ctrl_create_handle          0x00015220   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    i.hal_dsi_rx_ctrl_dcs_async_handler      0x00015260   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler)
    i.hal_dsi_rx_ctrl_deinit                 0x000152a0   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit)
    i.hal_dsi_rx_ctrl_get_max_ret_size       0x00015334   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size)
    i.hal_dsi_rx_ctrl_init                   0x00015354   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    i.hal_dsi_rx_ctrl_init_clk               0x00015400   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    hal_dsi_rx_ctrl_init_clk                 0x00015401   Thumb Code   222  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    i.hal_dsi_rx_ctrl_init_dsi_rx            0x00015500   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    hal_dsi_rx_ctrl_init_dsi_rx              0x00015501   Thumb Code   218  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    i.hal_dsi_rx_ctrl_init_memc              0x000155f8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    hal_dsi_rx_ctrl_init_memc                0x000155f9   Thumb Code   294  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    i.hal_dsi_rx_ctrl_init_rxbr              0x00015724   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    hal_dsi_rx_ctrl_init_rxbr                0x00015725   Thumb Code   314  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    i.hal_dsi_rx_ctrl_init_vidc              0x0001586c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    hal_dsi_rx_ctrl_init_vidc                0x0001586d   Thumb Code   624  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    i.hal_dsi_rx_ctrl_pre_init_pps           0x00015aec   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    i.hal_dsi_rx_ctrl_send_ack_cmd           0x00015b24   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd)
    i.hal_dsi_rx_ctrl_set_ipi_cfg            0x00015c14   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    hal_dsi_rx_ctrl_set_ipi_cfg              0x00015c15   Thumb Code    48  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    i.hal_dsi_rx_ctrl_start                  0x00015c44   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    i.hal_dsi_rx_ctrl_stop                   0x00015c74   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop)
    i.hal_dsi_rx_ctrl_toggle_resolution      0x00015ca4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    i.hal_dsi_tx_cmd_mode_cal_timing         0x00015cc4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing)
    hal_dsi_tx_cmd_mode_cal_timing           0x00015cc5   Thumb Code   506  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing)
    i.hal_dsi_tx_ctrl_create_handle          0x00015f40   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    i.hal_dsi_tx_ctrl_deinit                 0x00015f78   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit)
    i.hal_dsi_tx_ctrl_gen_a_tear_signal      0x00015fec   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal)
    i.hal_dsi_tx_ctrl_init                   0x00016010   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    i.hal_dsi_tx_ctrl_init_clk               0x0001608c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    hal_dsi_tx_ctrl_init_clk                 0x0001608d   Thumb Code    12  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    i.hal_dsi_tx_ctrl_set_overwrite_rgb      0x0001609c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    i.hal_dsi_tx_ctrl_set_tear_mode          0x000160a4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode)
    i.hal_dsi_tx_ctrl_start                  0x000160b0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    i.hal_dsi_tx_ctrl_stop                   0x0001612c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop)
    i.hal_dsi_tx_ctrl_write_array_cmd        0x00016164   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd)
    i.hal_dsi_tx_ctrl_write_cmd              0x00016258   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    i.hal_dsi_tx_init_cfg                    0x00016328   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg)
    hal_dsi_tx_init_cfg                      0x00016329   Thumb Code   258  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg)
    i.hal_dsi_tx_init_dpi_timing             0x00016434   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing)
    hal_dsi_tx_init_dpi_timing               0x00016435   Thumb Code    46  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing)
    i.hal_dsi_tx_init_phy_cfg                0x0001646c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    hal_dsi_tx_init_phy_cfg                  0x0001646d   Thumb Code    22  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    i.hal_dsi_tx_init_timing                 0x00016482   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing)
    hal_dsi_tx_init_timing                   0x00016483   Thumb Code    82  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing)
    i.hal_dsi_tx_init_vid_timing             0x000164d4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing)
    hal_dsi_tx_init_vid_timing               0x000164d5   Thumb Code    70  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing)
    i.hal_dsi_tx_send_cmd                    0x00016528   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    hal_dsi_tx_send_cmd                      0x00016529   Thumb Code    58  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    i.hal_dsi_tx_timing_info_update          0x00016568   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update)
    hal_dsi_tx_timing_info_update            0x00016569   Thumb Code   142  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update)
    i.hal_dsi_tx_vid_mode_cal_timing         0x000165fc   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing)
    hal_dsi_tx_vid_mode_cal_timing           0x000165fd   Thumb Code   766  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing)
    i.hal_gpio_config_pad                    0x0001690c   Section        0  hal_gpio.o(i.hal_gpio_config_pad)
    i.hal_gpio_ctrl_eint                     0x00016948   Section        0  hal_gpio.o(i.hal_gpio_ctrl_eint)
    i.hal_gpio_init_eint                     0x00016960   Section        0  hal_gpio.o(i.hal_gpio_init_eint)
    i.hal_gpio_init_input                    0x000169a0   Section        0  hal_gpio.o(i.hal_gpio_init_input)
    i.hal_gpio_init_output                   0x000169b6   Section        0  hal_gpio.o(i.hal_gpio_init_output)
    i.hal_gpio_reg_eint_cb                   0x000169d4   Section        0  hal_gpio.o(i.hal_gpio_reg_eint_cb)
    i.hal_gpio_set_ap_reset_int              0x000169f0   Section        0  hal_gpio.o(i.hal_gpio_set_ap_reset_int)
    i.hal_gpio_set_high_impedance            0x00016a40   Section        0  hal_gpio.o(i.hal_gpio_set_high_impedance)
    i.hal_gpio_set_mode                      0x00016a60   Section        0  hal_gpio.o(i.hal_gpio_set_mode)
    i.hal_gpio_set_output_data               0x00016ac4   Section        0  hal_gpio.o(i.hal_gpio_set_output_data)
    i.hal_gpio_set_pull_state                0x00016acc   Section        0  hal_gpio.o(i.hal_gpio_set_pull_state)
    i.hal_internal_sync_get_hight_performan_mode 0x00016b14   Section        0  hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode)
    i.hal_internal_sync_input_resolution_change 0x00016b24   Section        0  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    i.hal_internal_sync_register_lcdc_cb     0x00016cd8   Section        0  hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb)
    i.hal_internal_vsync_deinit              0x00016ce4   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    i.hal_internal_vsync_get_rx_state        0x00016d04   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state)
    i.hal_internal_vsync_get_sync_line       0x00016d10   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    i.hal_internal_vsync_get_tx_state        0x00016d24   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    i.hal_internal_vsync_init_rx             0x00016d30   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    i.hal_internal_vsync_init_tx             0x00016e08   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    i.hal_internal_vsync_set_rx_state        0x00016ed0   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    i.hal_internal_vsync_set_tear_mode       0x00016ef0   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    i.hal_internal_vsync_set_tx_state        0x00017008   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    i.hal_intl_dcs_init_sw_fltr              0x00017074   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr)
    i.hal_intl_dcs_rx_get_dcs_packet_data    0x000170e0   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data)
    hal_intl_dcs_rx_get_dcs_packet_data      0x000170e1   Thumb Code   806  hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data)
    i.hal_intl_dcs_rx_receive_packet         0x0001752c   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet)
    hal_intl_dcs_rx_receive_packet           0x0001752d   Thumb Code   122  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet)
    i.hal_intl_dcs_rx_receive_pps            0x000175b4   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps)
    hal_intl_dcs_rx_receive_pps              0x000175b5   Thumb Code   268  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps)
    i.hal_intl_dcs_set_auto_hw_filter        0x00017728   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter)
    i.hal_intl_dcs_sw_filter_handle          0x000177b4   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle)
    hal_intl_dcs_sw_filter_handle            0x000177b5   Thumb Code    36  hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle)
    i.hal_intl_fb_cal_fb_info                0x000177e0   Section        0  hal_internal_fb.o(i.hal_intl_fb_cal_fb_info)
    i.hal_intl_fb_check_bandwidth            0x00017ad0   Section        0  hal_internal_fb.o(i.hal_intl_fb_check_bandwidth)
    hal_intl_fb_check_bandwidth              0x00017ad1   Thumb Code    92  hal_internal_fb.o(i.hal_intl_fb_check_bandwidth)
    i.hal_intl_fb_edge_resize                0x00017b34   Section        0  hal_internal_fb.o(i.hal_intl_fb_edge_resize)
    hal_intl_fb_edge_resize                  0x00017b35   Thumb Code   214  hal_internal_fb.o(i.hal_intl_fb_edge_resize)
    i.hal_intl_fb_flow_control_adapter       0x00017c10   Section        0  hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter)
    hal_intl_fb_flow_control_adapter         0x00017c11   Thumb Code    94  hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter)
    i.hal_intl_fb_get_memc_flow_mode         0x00017c74   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode)
    i.hal_intl_fb_get_rx_fb_info             0x00017c80   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info)
    i.hal_intl_fb_get_tx_fb_info             0x00017c90   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info)
    i.hal_intl_fb_get_user_flow              0x00017ca0   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_user_flow)
    i.hal_intl_svs_deinit_rx                 0x00017cac   Section        0  hal_internal_svs.o(i.hal_intl_svs_deinit_rx)
    i.hal_intl_svs_deinit_tx                 0x00017cd4   Section        0  hal_internal_svs.o(i.hal_intl_svs_deinit_tx)
    i.hal_intl_svs_handle                    0x00017ce4   Section        0  hal_internal_svs.o(i.hal_intl_svs_handle)
    i.hal_intl_svs_init_rx                   0x00017d08   Section        0  hal_internal_svs.o(i.hal_intl_svs_init_rx)
    i.hal_intl_svs_init_tx                   0x00017d88   Section        0  hal_internal_svs.o(i.hal_intl_svs_init_tx)
    i.hal_intl_svs_set_rx_vtt                0x00017d9c   Section        0  hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt)
    i.hal_intl_svs_update_rxbr_clk           0x00017da8   Section        0  hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk)
    i.hal_lcdc_displayproc_config            0x00017df0   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config)
    i.hal_lcdc_init_cfg                      0x00017e60   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    hal_lcdc_init_cfg                        0x00017e61   Thumb Code    62  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    i.hal_lcdc_init_clk                      0x00017e9e   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    hal_lcdc_init_clk                        0x00017e9f   Thumb Code   112  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    i.hal_lcdc_postproc_config               0x00017f10   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config)
    i.hal_lcdc_start                         0x00018038   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_start)
    hal_lcdc_start                           0x00018039   Thumb Code    36  hal_dsi_tx_ctrl.o(i.hal_lcdc_start)
    i.hal_lcdc_timinggen_config              0x0001805c   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config)
    hal_lcdc_timinggen_config                0x0001805d   Thumb Code    60  hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config)
    i.hal_lcdc_upscaler_config               0x00018098   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config)
    i.hal_nonshadow_func_update              0x00018178   Section        0  hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update)
    i.hal_pwr_enter_deep_sleep_mode          0x00018234   Section        0  hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode)
    i.hal_pwr_enter_normal_sleep_mode        0x0001825e   Section        0  hal_pwr.o(i.hal_pwr_enter_normal_sleep_mode)
    i.hal_pwr_enter_stop_sleep_mode          0x00018268   Section        0  hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode)
    i.hal_pwr_exit_sleep_mode                0x000182cc   Section        0  hal_pwr.o(i.hal_pwr_exit_sleep_mode)
    i.hal_pwr_get_vcc_power_ready            0x000182d6   Section        0  hal_pwr.o(i.hal_pwr_get_vcc_power_ready)
    i.hal_pwr_set_main_power                 0x000182de   Section        0  hal_pwr.o(i.hal_pwr_set_main_power)
    i.hal_pwr_set_sleep_mode_power           0x000182e6   Section        0  hal_pwr.o(i.hal_pwr_set_sleep_mode_power)
    i.hal_pwr_set_stop_sleep_wakeup_pin      0x000182f0   Section        0  hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin)
    i.hal_swire_deinit                       0x00018354   Section        0  hal_swire.o(i.hal_swire_deinit)
    i.hal_swire_enable                       0x00018394   Section        0  hal_swire.o(i.hal_swire_enable)
    i.hal_swire_init                         0x000183f0   Section        0  hal_swire.o(i.hal_swire_init)
    i.hal_swire_set_pulse                    0x00018448   Section        0  hal_swire.o(i.hal_swire_set_pulse)
    i.hal_swire_set_timer                    0x0001846c   Section        0  hal_swire.o(i.hal_swire_set_timer)
    i.hal_system_init                        0x000184ac   Section        0  hal_system.o(i.hal_system_init)
    i.hal_system_updata_sysclk               0x00018590   Section        0  hal_system.o(i.hal_system_updata_sysclk)
    i.hal_timer_deinit                       0x000185e0   Section        0  hal_timer.o(i.hal_timer_deinit)
    i.hal_timer_init                         0x00018610   Section        0  hal_timer.o(i.hal_timer_init)
    i.hal_timer_set_repeat                   0x0001862c   Section        0  hal_timer.o(i.hal_timer_set_repeat)
    i.hal_tx_frame_rate_adjust               0x00018634   Section        0  hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust)
    hal_tx_frame_rate_adjust                 0x00018635   Thumb Code    44  hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust)
    i.hal_uart_init                          0x00018664   Section        0  hal_uart.o(i.hal_uart_init)
    i.hal_uart_send_blocking                 0x000186f8   Section        0  hal_uart.o(i.hal_uart_send_blocking)
    i.hal_vsync_func_update                  0x00018714   Section        0  hal_dsi_tx_ctrl.o(i.hal_vsync_func_update)
    i.hal_vsync_reset_lcdc_scaler            0x0001872c   Section        0  hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler)
    i.main                                   0x000187f8   Section        0  main.o(i.main)
    i.pps_update_handle                      0x00018838   Section        0  p6a_demo.o(i.pps_update_handle)
    pps_update_handle                        0x00018839   Thumb Code   110  p6a_demo.o(i.pps_update_handle)
    i.rxbr_irq1_callback                     0x000188b4   Section        0  hal_internal_vsync.o(i.rxbr_irq1_callback)
    rxbr_irq1_callback                       0x000188b5   Thumb Code   466  hal_internal_vsync.o(i.rxbr_irq1_callback)
    i.send_panel_init_code                   0x00018b6c   Section        0  p6a_demo.o(i.send_panel_init_code)
    send_panel_init_code                     0x00018b6d   Thumb Code    58  p6a_demo.o(i.send_panel_init_code)
    i.soft_double_buffer_update              0x00018ba8   Section        0  hal_internal_vsync.o(i.soft_double_buffer_update)
    soft_double_buffer_update                0x00018ba9   Thumb Code    56  hal_internal_vsync.o(i.soft_double_buffer_update)
    i.soft_gen_te                            0x00018bec   Section        0  hal_internal_vsync.o(i.soft_gen_te)
    soft_gen_te                              0x00018bed   Thumb Code   102  hal_internal_vsync.o(i.soft_gen_te)
    i.soft_gen_te_double_buffer              0x00018c68   Section        0  hal_internal_vsync.o(i.soft_gen_te_double_buffer)
    soft_gen_te_double_buffer                0x00018c69   Thumb Code   122  hal_internal_vsync.o(i.soft_gen_te_double_buffer)
    i.stop_sleep_cb                          0x00018cfc   Section        0  hal_pwr.o(i.stop_sleep_cb)
    stop_sleep_cb                            0x00018cfd   Thumb Code    18  hal_pwr.o(i.stop_sleep_cb)
    i.svs_direct_mode_setting                0x00018d14   Section        0  hal_internal_svs.o(i.svs_direct_mode_setting)
    svs_direct_mode_setting                  0x00018d15   Thumb Code   154  hal_internal_svs.o(i.svs_direct_mode_setting)
    i.svs_get_rel_intv                       0x00018dc0   Section        0  hal_internal_svs.o(i.svs_get_rel_intv)
    svs_get_rel_intv                         0x00018dc1   Thumb Code    20  hal_internal_svs.o(i.svs_get_rel_intv)
    i.svs_sync_handle                        0x00018ddc   Section        0  hal_internal_svs.o(i.svs_sync_handle)
    svs_sync_handle                          0x00018ddd   Thumb Code   158  hal_internal_svs.o(i.svs_sync_handle)
    i.svs_wait_fr_stab                       0x00018e8c   Section        0  hal_internal_svs.o(i.svs_wait_fr_stab)
    svs_wait_fr_stab                         0x00018e8d   Thumb Code   148  hal_internal_svs.o(i.svs_wait_fr_stab)
    i.svs_wait_start                         0x00018f58   Section        0  hal_internal_svs.o(i.svs_wait_start)
    svs_wait_start                           0x00018f59   Thumb Code   250  hal_internal_svs.o(i.svs_wait_start)
    i.tau_log_init                           0x00019064   Section        0  tau_log.o(i.tau_log_init)
    i.tau_log_printf                         0x00019098   Section        0  tau_log.o(i.tau_log_printf)
    i.tau_log_push_log                       0x0001911c   Section        0  tau_log.o(i.tau_log_push_log)
    i.vidc_callback                          0x00019194   Section        0  hal_internal_vsync.o(i.vidc_callback)
    vidc_callback                            0x00019195   Thumb Code   150  hal_internal_vsync.o(i.vidc_callback)
    i.vpre_err_reset                         0x00019248   Section        0  hal_internal_vsync.o(i.vpre_err_reset)
    vpre_err_reset                           0x00019249   Thumb Code   254  hal_internal_vsync.o(i.vpre_err_reset)
    .constdata                               0x00019360   Section     8364  p6a_demo.o(.constdata)
    g_cus_rx_dcs_execute_table               0x00019360   Data          96  p6a_demo.o(.constdata)
    .constdata                               0x0001b40c   Section       40  hal_dsi_rx_ctrl.o(.constdata)
    .constdata                               0x0001b434   Section       28  hal_dsi_tx_ctrl.o(.constdata)
    .constdata                               0x0001b450   Section       78  hal_gpio.o(.constdata)
    s_gpio_perf                              0x0001b450   Data          78  hal_gpio.o(.constdata)
    .constdata                               0x0001b4a0   Section       48  hal_uart.o(.constdata)
    .constdata                               0x0001b4d0   Section       16  drv_uart.o(.constdata)
    .conststring                             0x0001b4e0   Section       66  hal_dsi_rx_ctrl.o(.conststring)
    .conststring                             0x0001b524   Section      144  hal_internal_vsync.o(.conststring)
    .conststring                             0x0001b5b4   Section      142  hal_internal_dcs.o(.conststring)
    .data                                    0x00070000   Section      287  p6a_demo.o(.data)
    g_rx_ctrl_handle                         0x00070000   Data           4  p6a_demo.o(.data)
    g_tx_ctrl_handle                         0x00070004   Data           4  p6a_demo.o(.data)
    panel_display_done                       0x00070008   Data           1  p6a_demo.o(.data)
    sg_system_resume                         0x00070009   Data           1  p6a_demo.o(.data)
    sg_system_suspend                        0x0007000a   Data           1  p6a_demo.o(.data)
    sg_exit_idle_mode_flag                   0x0007000b   Data           1  p6a_demo.o(.data)
    g_resolution_change                      0x0007000c   Data           1  p6a_demo.o(.data)
    pps_renew_flag                           0x00070010   Data           4  p6a_demo.o(.data)
    pwr_rst_flag                             0x00070014   Data           4  p6a_demo.o(.data)
    reg53_E8_fg                              0x0007011e   Data           1  p6a_demo.o(.data)
    .data                                    0x00070120   Section       36  hal_dsi_rx_ctrl.o(.data)
    g_hw_auto_filter                         0x00070120   Data           1  hal_dsi_rx_ctrl.o(.data)
    g_crc_check_enable                       0x00070121   Data           1  hal_dsi_rx_ctrl.o(.data)
    g_esc_clk                                0x00070124   Data           4  hal_dsi_rx_ctrl.o(.data)
    g_before_draw_col                        0x00070128   Data           4  hal_dsi_rx_ctrl.o(.data)
    g_before_draw_page                       0x0007012c   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_step                                 0x00070130   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_cmd_filter                           0x00070134   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_x                                    0x00070138   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_y                                    0x0007013c   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_value                                0x00070140   Data           4  hal_dsi_rx_ctrl.o(.data)
    .data                                    0x00070144   Section       92  hal_dsi_tx_ctrl.o(.data)
    sg_bta_vsync_flag                        0x00070144   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_vsync_flag                            0x00070145   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_enter_sleep_cmd                       0x00070146   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_fldc_cg_mode                          0x00070147   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_scl_fir                        0x00070148   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_honly_bypass_fir                      0x00070149   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_bcs                            0x0007014a   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_enhc                           0x0007014b   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_edge_dect                      0x0007014c   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_edge_enh                       0x0007014d   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_dith                           0x0007014e   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_dith_judge                            0x0007014f   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_endianness                            0x00070150   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_test_pattern_en                       0x00070151   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_dith_judge_thr                        0x00070154   Data           4  hal_dsi_tx_ctrl.o(.data)
    sg_ccm_para                              0x00070158   Data          36  hal_dsi_tx_ctrl.o(.data)
    sg_honly_para                            0x0007017c   Data          36  hal_dsi_tx_ctrl.o(.data)
    .data                                    0x000701a0   Section        2  hal_swire.o(.data)
    sg_swire_timer                           0x000701a0   Data           1  hal_swire.o(.data)
    sg_swire_repeat                          0x000701a1   Data           1  hal_swire.o(.data)
    .data                                    0x000701a4   Section        8  hal_pwr.o(.data)
    sg_wake_up_io                            0x000701a4   Data           1  hal_pwr.o(.data)
    sg_stop_sleep_wakeup_int                 0x000701a8   Data           4  hal_pwr.o(.data)
    .data                                    0x000701ac   Section        1  tau_log.o(.data)
    g_log_port                               0x000701ac   Data           1  tau_log.o(.data)
    .data                                    0x000701b0   Section       24  hal_uart.o(.data)
    sg_dma_callback                          0x000701c0   Data           4  hal_uart.o(.data)
    sg_user_data                             0x000701c4   Data           4  hal_uart.o(.data)
    .data                                    0x000701c8   Section       16  hal_internal_vsync.o(.data)
    s_te_refine_mode                         0x000701c8   Data           1  hal_internal_vsync.o(.data)
    s_double_buffer                          0x000701c9   Data           1  hal_internal_vsync.o(.data)
    .data                                    0x000701d8   Section       40  hal_internal_dcs.o(.data)
    pre_nslc                                 0x000701d8   Data           4  hal_internal_dcs.o(.data)
    g_imm_packet                             0x000701dc   Data          24  hal_internal_dcs.o(.data)
    g_cus_rx_write_cmd_handle                0x000701f4   Data          12  hal_internal_dcs.o(.data)
    .data                                    0x00070200   Section       12  drv_common.o(.data)
    s_my_tick                                0x00070200   Data           4  drv_common.o(.data)
    .data                                    0x0007020c   Section        1  drv_common.o(.data)
    .data                                    0x00070210   Section        4  drv_gpio.o(.data)
    g_ap_reset_cb                            0x00070210   Data           4  drv_gpio.o(.data)
    .data                                    0x00070214   Section        4  drv_swire.o(.data)
    sg_drv_swire_cb                          0x00070214   Data           4  drv_swire.o(.data)
    .data                                    0x00070218   Section       80  drv_timer.o(.data)
    sg_timer_info                            0x00070218   Data          80  drv_timer.o(.data)
    .data                                    0x00070268   Section        4  drv_se.o(.data)
    chip_info                                0x00070268   Data           4  drv_se.o(.data)
    .data                                    0x0007026c   Section        1  drv_dsi_rx.o(.data)
    sg_rx_drv_level                          0x0007026c   Data           1  drv_dsi_rx.o(.data)
    .data                                    0x00070270   Section        8  drv_rxbr.o(.data)
    .data                                    0x00070278   Section        4  drv_vidc.o(.data)
    .data                                    0x0007027c   Section      400  drv_dma.o(.data)
    sg_dma_handle                            0x0007027c   Data         256  drv_dma.o(.data)
    .data                                    0x0007040c   Section        4  stdout.o(.data)
    .bss                                     0x00070410   Section      208  hal_dsi_rx_ctrl.o(.bss)
    g_rx_ctrl_handle                         0x00070410   Data         208  hal_dsi_rx_ctrl.o(.bss)
    .bss                                     0x000704e0   Section      184  hal_dsi_tx_ctrl.o(.bss)
    g_tx_ctrl_handle                         0x000704e0   Data          92  hal_dsi_tx_ctrl.o(.bss)
    sg_dsi_tx_param                          0x0007053c   Data          92  hal_dsi_tx_ctrl.o(.bss)
    .bss                                     0x00070598   Section      256  tau_log.o(.bss)
    g_log_buf                                0x00070598   Data         256  tau_log.o(.bss)
    .bss                                     0x00070698   Section       40  hal_internal_vsync.o(.bss)
    .bss                                     0x000706c0   Section     2048  hal_internal_dcs.o(.bss)
    .bss                                     0x00070ec0   Section      255  hal_internal_dcs.o(.bss)
    g_imm_buffer                             0x00070ec0   Data         255  hal_internal_dcs.o(.bss)
    .bss                                     0x00070fc0   Section       68  hal_internal_fb.o(.bss)
    .bss                                     0x00071004   Section       68  hal_internal_svs.o(.bss)
    sg_sys_handler                           0x00071004   Data          68  hal_internal_svs.o(.bss)
    .bss                                     0x00071048   Section       64  drv_gpio.o(.bss)
    s_gpio_cb                                0x00071048   Data          64  drv_gpio.o(.bss)
    .bss                                     0x00071088   Section     4204  dcs_packet_fifo.o(.bss)
    .bss                                     0x000720f4   Section       16  drv_dma.o(.bss)
    sg_dma_int_list                          0x000720f4   Data          16  drv_dma.o(.bss)
    .bss                                     0x00072104   Section       96  drv_uart.o(.bss)
    sg_uart_userdata                         0x00072104   Data          96  drv_uart.o(.bss)
    STACK                                    0x00072168   Section     4096  startup_armcm0.o(STACK)

    Global Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    BuildAttributes$$THM_ISAv3M$S$PE$A:L22$X:L11$S22$IEEE1$IW$USESV6$~STKCKD$USESV7$~SHL$OTIME$ROPI$IEEEJ$EBA8$MICROLIB$REQ8$PRES8$EABIv2 0x00000000   Number         0  anon$$obj.o ABSOLUTE
    __ARM_use_no_argv                        0x00000000   Number         0  main.o ABSOLUTE
    _printf_a                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_c                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_charcount                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_d                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_e                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_f                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_flags                            0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_dec                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_hex                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_g                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_i                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_int_dec                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_l                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ll                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lld                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lli                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llo                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llu                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llx                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_dec                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_hex                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_oct                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ls                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_mbtowc                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_n                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_o                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_p                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_percent                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_pre_padding                      0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_return_value                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_s                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_sizespec                         0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_str                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_signed                  0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_unsigned                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_u                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wctomb                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_widthprec                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_x                                0x00000000   Number         0  stubs.o ABSOLUTE
    __cpp_initialize__aeabi_                  - Undefined Weak Reference
    __cxa_finalize                            - Undefined Weak Reference
    _clock_init                               - Undefined Weak Reference
    _microlib_exit                            - Undefined Weak Reference
    __Vectors_Size                           0x000000c0   Number         0  startup_armcm0.o ABSOLUTE
    __Vectors                                0x00010000   Data           4  startup_armcm0.o(RESET)
    __Vectors_End                            0x000100c0   Data           0  startup_armcm0.o(RESET)
    __main                                   0x000100c1   Thumb Code     0  entry.o(.ARM.Collect$$$$00000000)
    _main_stk                                0x000100c1   Thumb Code     0  entry2.o(.ARM.Collect$$$$00000001)
    _main_scatterload                        0x000100c5   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    __main_after_scatterload                 0x000100c9   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    _main_clock                              0x000100c9   Thumb Code     0  entry7b.o(.ARM.Collect$$$$00000008)
    _main_cpp_init                           0x000100c9   Thumb Code     0  entry8b.o(.ARM.Collect$$$$0000000A)
    _main_init                               0x000100c9   Thumb Code     0  entry9a.o(.ARM.Collect$$$$0000000B)
    __rt_final_cpp                           0x000100d1   Thumb Code     0  entry10a.o(.ARM.Collect$$$$0000000D)
    __rt_final_exit                          0x000100d1   Thumb Code     0  entry11a.o(.ARM.Collect$$$$0000000F)
    Reset_Handler                            0x000100d5   Thumb Code    28  startup_armcm0.o(.text)
    NMI_Handler                              0x000100f1   Thumb Code     2  startup_armcm0.o(.text)
    SVC_Handler                              0x000100f5   Thumb Code     2  startup_armcm0.o(.text)
    PendSV_Handler                           0x000100f7   Thumb Code     2  startup_armcm0.o(.text)
    FLSCTRL_IRQn_Handler                     0x00010107   Thumb Code     2  startup_armcm0.o(.text)
    WDG_IRQn_Handler                         0x00010113   Thumb Code     2  startup_armcm0.o(.text)
    I2C0_IRQn_Handler                        0x00010117   Thumb Code     2  startup_armcm0.o(.text)
    I2C1_IRQn_Handler                        0x00010119   Thumb Code     2  startup_armcm0.o(.text)
    SPIS_IRQn_Handler                        0x0001011b   Thumb Code     2  startup_armcm0.o(.text)
    SPIM_IRQn_Handler                        0x0001011d   Thumb Code     2  startup_armcm0.o(.text)
    I2C2_IRQn_Handler                        0x00010121   Thumb Code     2  startup_armcm0.o(.text)
    OTP_IRQn_Handler                         0x00010123   Thumb Code     2  startup_armcm0.o(.text)
    PVD_IRQn_Handler                         0x00010127   Thumb Code     2  startup_armcm0.o(.text)
    __aeabi_uidiv                            0x0001014d   Thumb Code     0  uidiv.o(.text)
    __aeabi_uidivmod                         0x0001014d   Thumb Code    44  uidiv.o(.text)
    __aeabi_idiv                             0x00010179   Thumb Code     0  idiv.o(.text)
    __aeabi_idivmod                          0x00010179   Thumb Code    40  idiv.o(.text)
    __aeabi_memcpy                           0x000101a1   Thumb Code    36  memcpya.o(.text)
    __aeabi_memcpy4                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memcpy8                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memset                           0x000101c5   Thumb Code    14  memseta.o(.text)
    __aeabi_memset4                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memset8                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr                           0x000101d3   Thumb Code     4  memseta.o(.text)
    __aeabi_memclr4                          0x000101d3   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr8                          0x000101d3   Thumb Code     0  memseta.o(.text)
    _memset$wrapper                          0x000101d7   Thumb Code    18  memseta.o(.text)
    strlen                                   0x000101e9   Thumb Code    14  strlen.o(.text)
    __aeabi_fadd                             0x000101f7   Thumb Code   162  fadd.o(.text)
    __aeabi_fsub                             0x00010299   Thumb Code     8  fadd.o(.text)
    __aeabi_frsub                            0x000102a1   Thumb Code     8  fadd.o(.text)
    __aeabi_fmul                             0x000102a9   Thumb Code   122  fmul.o(.text)
    __aeabi_fdiv                             0x00010323   Thumb Code   124  fdiv.o(.text)
    __ARM_scalbnf                            0x0001039f   Thumb Code    24  fscalb.o(.text)
    scalbnf                                  0x0001039f   Thumb Code     0  fscalb.o(.text)
    __aeabi_dadd                             0x000103b9   Thumb Code   328  dadd.o(.text)
    __aeabi_dsub                             0x00010501   Thumb Code    12  dadd.o(.text)
    __aeabi_drsub                            0x0001050d   Thumb Code    12  dadd.o(.text)
    __aeabi_dmul                             0x0001051d   Thumb Code   202  dmul.o(.text)
    __aeabi_ui2f                             0x000105ed   Thumb Code    14  ffltui.o(.text)
    __aeabi_ui2d                             0x000105fd   Thumb Code    24  dfltui.o(.text)
    __aeabi_f2uiz                            0x00010619   Thumb Code    40  ffixui.o(.text)
    __aeabi_d2uiz                            0x00010641   Thumb Code    50  dfixui.o(.text)
    __aeabi_f2d                              0x0001067d   Thumb Code    40  f2d.o(.text)
    __aeabi_d2f                              0x000106a5   Thumb Code    56  d2f.o(.text)
    __aeabi_cfcmpeq                          0x000106dd   Thumb Code     0  cfcmple.o(.text)
    __aeabi_cfcmple                          0x000106dd   Thumb Code    20  cfcmple.o(.text)
    __aeabi_cfrcmple                         0x000106f1   Thumb Code    20  cfrcmple.o(.text)
    __aeabi_uldivmod                         0x00010705   Thumb Code    96  uldiv.o(.text)
    __aeabi_llsl                             0x00010765   Thumb Code    32  llshl.o(.text)
    _ll_shift_l                              0x00010765   Thumb Code     0  llshl.o(.text)
    __aeabi_llsr                             0x00010785   Thumb Code    34  llushr.o(.text)
    _ll_ushift_r                             0x00010785   Thumb Code     0  llushr.o(.text)
    __aeabi_lasr                             0x000107a7   Thumb Code    38  llsshr.o(.text)
    _ll_sshift_r                             0x000107a7   Thumb Code     0  llsshr.o(.text)
    __I$use$fp                               0x000107cd   Thumb Code     0  iusefp.o(.text)
    _float_round                             0x000107cd   Thumb Code    16  fepilogue.o(.text)
    _float_epilogue                          0x000107dd   Thumb Code   114  fepilogue.o(.text)
    _double_round                            0x0001084f   Thumb Code    26  depilogue.o(.text)
    _double_epilogue                         0x00010869   Thumb Code   164  depilogue.o(.text)
    __aeabi_ddiv                             0x0001090d   Thumb Code   234  ddiv.o(.text)
    __aeabi_d2ulz                            0x000109fd   Thumb Code    54  dfixul.o(.text)
    __aeabi_cdrcmple                         0x00010a3d   Thumb Code    38  cdrcmple.o(.text)
    __scatterload                            0x00010a65   Thumb Code    28  init.o(.text)
    __scatterload_rt2                        0x00010a65   Thumb Code     0  init.o(.text)
    __decompress                             0x00010a89   Thumb Code     0  __dczerorl2.o(.text)
    __decompress1                            0x00010a89   Thumb Code    86  __dczerorl2.o(.text)
    AP_NRESET_IRQn_Handler                   0x00010ae1   Thumb Code    22  drv_gpio.o(i.AP_NRESET_IRQn_Handler)
    DMA_IRQn_Handler                         0x00010afd   Thumb Code    78  drv_dma.o(i.DMA_IRQn_Handler)
    EXTI_INT0_IRQn_Handler                   0x00010b59   Thumb Code    10  drv_gpio.o(i.EXTI_INT0_IRQn_Handler)
    EXTI_INT1_IRQn_Handler                   0x00010b63   Thumb Code    10  drv_gpio.o(i.EXTI_INT1_IRQn_Handler)
    EXTI_INT2_IRQn_Handler                   0x00010b6d   Thumb Code    10  drv_gpio.o(i.EXTI_INT2_IRQn_Handler)
    EXTI_INT3_IRQn_Handler                   0x00010b77   Thumb Code    10  drv_gpio.o(i.EXTI_INT3_IRQn_Handler)
    EXTI_INT4_IRQn_Handler                   0x00010b81   Thumb Code    10  drv_gpio.o(i.EXTI_INT4_IRQn_Handler)
    EXTI_INT5_IRQn_Handler                   0x00010b8b   Thumb Code    10  drv_gpio.o(i.EXTI_INT5_IRQn_Handler)
    EXTI_INT6_IRQn_Handler                   0x00010b95   Thumb Code    10  drv_gpio.o(i.EXTI_INT6_IRQn_Handler)
    EXTI_INT7_IRQn_Handler                   0x00010b9f   Thumb Code    10  drv_gpio.o(i.EXTI_INT7_IRQn_Handler)
    HardFault_Handler                        0x00010ba9   Thumb Code    14  drv_common.o(i.HardFault_Handler)
    LCDC_IRQn_Handler                        0x00010bf1   Thumb Code   118  hal_internal_vsync.o(i.LCDC_IRQn_Handler)
    MEMC_IRQn_Handler                        0x00010cf1   Thumb Code   154  drv_memc.o(i.MEMC_IRQn_Handler)
    MIPI_TX_IRQn_Handler                     0x00010d8d   Thumb Code    70  drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler)
    SWIRE_IRQn_Handler                       0x00010e45   Thumb Code    38  drv_swire.o(i.SWIRE_IRQn_Handler)
    SysTick_Handler                          0x00010e75   Thumb Code    20  drv_common.o(i.SysTick_Handler)
    TIMER0_IRQn_Handler                      0x00010e8d   Thumb Code    10  drv_timer.o(i.TIMER0_IRQn_Handler)
    TIMER1_IRQn_Handler                      0x00010e97   Thumb Code    10  drv_timer.o(i.TIMER1_IRQn_Handler)
    TIMER2_IRQn_Handler                      0x00010ea1   Thumb Code    10  drv_timer.o(i.TIMER2_IRQn_Handler)
    TIMER3_IRQn_Handler                      0x00010eab   Thumb Code    10  drv_timer.o(i.TIMER3_IRQn_Handler)
    VIDC_IRQn_Handler                        0x00010eb5   Thumb Code    22  drv_vidc.o(i.VIDC_IRQn_Handler)
    VPRE1_IRQn_Handler                       0x00010ed1   Thumb Code    22  drv_rxbr.o(i.VPRE1_IRQn_Handler)
    VPRE_IRQn_Handler                        0x00010eed   Thumb Code   116  hal_internal_dcs.o(i.VPRE_IRQn_Handler)
    __0printf                                0x00010f69   Thumb Code    24  printfa.o(i.__0printf)
    __1printf                                0x00010f69   Thumb Code     0  printfa.o(i.__0printf)
    __2printf                                0x00010f69   Thumb Code     0  printfa.o(i.__0printf)
    __c89printf                              0x00010f69   Thumb Code     0  printfa.o(i.__0printf)
    printf                                   0x00010f69   Thumb Code     0  printfa.o(i.__0printf)
    __0vsprintf                              0x00010f89   Thumb Code    30  printfa.o(i.__0vsprintf)
    __1vsprintf                              0x00010f89   Thumb Code     0  printfa.o(i.__0vsprintf)
    __2vsprintf                              0x00010f89   Thumb Code     0  printfa.o(i.__0vsprintf)
    __c89vsprintf                            0x00010f89   Thumb Code     0  printfa.o(i.__0vsprintf)
    vsprintf                                 0x00010f89   Thumb Code     0  printfa.o(i.__0vsprintf)
    __ARM_clz                                0x00010fad   Thumb Code    46  depilogue.o(i.__ARM_clz)
    __ARM_common_switch8                     0x00010fdb   Thumb Code    26  hal_dsi_rx_ctrl.o(i.__ARM_common_switch8)
    __scatterload_null                       0x00010ff5   Thumb Code     2  handlers.o(i.__scatterload_null)
    s_RAM_CK                                 0x00011000   Data          28  drv_common.o(.ARM.__at_0x11000)
    g_tau_log                                0x0001101c   Data          16  tau_log.o(.ARM.__at_0x1101C)
    sg_pq_para                               0x0001102c   Data          22  hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C)
    MIPI_RX_IRQn_Handler                     0x00011045   Thumb Code   354  drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler)
    UART_IRQn_Handler                        0x000113a9   Thumb Code   364  drv_uart.o(i.UART_IRQn_Handler)
    __scatterload_copy                       0x00011561   Thumb Code    14  handlers.o(i.__scatterload_copy)
    __scatterload_zeroinit                   0x0001156f   Thumb Code    14  handlers.o(i.__scatterload_zeroinit)
    app_display_init                         0x000122c3   Thumb Code    44  p6a_demo.o(i.app_display_init)
    app_gpio_init                            0x000122f1   Thumb Code    22  p6a_demo.o(i.app_gpio_init)
    board_Init                               0x00012875   Thumb Code    20  board.o(i.board_Init)
    ceil                                     0x0001288d   Thumb Code   180  ceil.o(i.ceil)
    dcs_packet_fifo_alloc                    0x00012a09   Thumb Code    80  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    dcs_packet_fifo_init                     0x00012a61   Thumb Code    18  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    dcs_packet_free_fifo_header              0x00012a79   Thumb Code    60  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    dcs_packet_get_fifo_header               0x00012abd   Thumb Code    26  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    delayMs                                  0x00012ae1   Thumb Code    24  tau_delay.o(i.delayMs)
    delayUs                                  0x00012af9   Thumb Code    40  tau_delay.o(i.delayUs)
    drv_common_system_init                   0x00012b25   Thumb Code     8  drv_common.o(i.drv_common_system_init)
    drv_crgu_enable_clock                    0x00012b2d   Thumb Code    54  drv_crgu.o(i.drv_crgu_enable_clock)
    drv_crgu_get_rxbr_clk                    0x00012b69   Thumb Code    70  drv_crgu.o(i.drv_crgu_get_rxbr_clk)
    drv_crgu_reset_modules                   0x00012bd1   Thumb Code    10  drv_crgu.o(i.drv_crgu_reset_modules)
    drv_crgu_set_ahb_clk                     0x00012be1   Thumb Code    34  drv_crgu.o(i.drv_crgu_set_ahb_clk)
    drv_crgu_set_clock_div                   0x00012c09   Thumb Code    12  drv_crgu.o(i.drv_crgu_set_clock_div)
    drv_crgu_set_dpi_clk                     0x00012c19   Thumb Code    54  drv_crgu.o(i.drv_crgu_set_dpi_clk)
    drv_crgu_set_dsc_clk                     0x00012c55   Thumb Code    52  drv_crgu.o(i.drv_crgu_set_dsc_clk)
    drv_crgu_set_fb_clk                      0x00012c8d   Thumb Code    34  drv_crgu.o(i.drv_crgu_set_fb_clk)
    drv_crgu_set_lcdc_clk                    0x00012cb5   Thumb Code    36  drv_crgu.o(i.drv_crgu_set_lcdc_clk)
    drv_crgu_set_reset                       0x00012cdd   Thumb Code    20  drv_crgu.o(i.drv_crgu_set_reset)
    drv_crgu_set_rxbr_clk                    0x00012cf5   Thumb Code    34  drv_crgu.o(i.drv_crgu_set_rxbr_clk)
    drv_crgu_set_vidc_clk                    0x00012d1d   Thumb Code    36  drv_crgu.o(i.drv_crgu_set_vidc_clk)
    drv_dma_clear_status                     0x00012d45   Thumb Code    20  drv_dma.o(i.drv_dma_clear_status)
    drv_dsc_dec_disable                      0x00012d71   Thumb Code    20  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    drv_dsc_dec_enable                       0x00012d8d   Thumb Code    44  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    drv_dsc_dec_get_nslc                     0x00012dc5   Thumb Code    22  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    drv_dsc_dec_set_irqen                    0x00012de5   Thumb Code    24  drv_dsc_dec.o(i.drv_dsc_dec_set_irqen)
    drv_dsi_rx_calc_ipi_tx_delay             0x00012e01   Thumb Code   252  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    drv_dsi_rx_enable_irq                    0x00012f0d   Thumb Code    58  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    drv_dsi_rx_get_compression_en            0x00012fb9   Thumb Code    10  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    drv_dsi_rx_get_ddi_crc_en                0x00012fc9   Thumb Code    10  drv_dsi_rx.o(i.drv_dsi_rx_get_ddi_crc_en)
    drv_dsi_rx_get_max_ret_size              0x00012fd9   Thumb Code     8  drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size)
    drv_dsi_rx_power_up                      0x00012fe5   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    drv_dsi_rx_set_check_crc                 0x00012ffd   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc)
    drv_dsi_rx_set_ctrl_cfg                  0x00013019   Thumb Code    32  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    drv_dsi_rx_set_ddi_cfg                   0x0001303d   Thumb Code    10  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    drv_dsi_rx_set_ddi_crc_en                0x0001304d   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_crc_en)
    drv_dsi_rx_set_inten                     0x00013069   Thumb Code     8  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    drv_dsi_rx_set_ipi_cfg                   0x00013075   Thumb Code    12  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    drv_dsi_rx_set_ipi_ycbcr_frmt            0x00013085   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_ycbcr_frmt)
    drv_dsi_rx_set_lane_swap                 0x000130a1   Thumb Code    16  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    drv_dsi_rx_set_resp_cnt                  0x000130b5   Thumb Code    32  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    drv_dsi_rx_set_tear_resp_en              0x000130d9   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_tear_resp_en)
    drv_dsi_rx_set_up_phy                    0x000130f5   Thumb Code   224  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    drv_dsi_rx_shut_down                     0x000131f5   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    drv_dsi_tx_command_header                0x0001320d   Thumb Code    18  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    drv_dsi_tx_command_mode_cfg              0x00013225   Thumb Code    82  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    drv_dsi_tx_command_put_payload           0x0001327d   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    drv_dsi_tx_config_eotp                   0x00013289   Thumb Code    26  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    drv_dsi_tx_config_int                    0x000132a9   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    drv_dsi_tx_dpi_lpcmd_time                0x000132b5   Thumb Code    10  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    drv_dsi_tx_dpi_mode                      0x000132c5   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    drv_dsi_tx_dpi_polarity                  0x000132d5   Thumb Code    32  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    drv_dsi_tx_edpi_cmd_size                 0x000132f9   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    drv_dsi_tx_get_cmd_status                0x00013305   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    drv_dsi_tx_mode                          0x00013311   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    drv_dsi_tx_phy_clock_lane_auto_lp        0x0001331d   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    drv_dsi_tx_phy_clock_lane_req_hs         0x00013339   Thumb Code    26  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    drv_dsi_tx_phy_lane_mode                 0x00013359   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    drv_dsi_tx_phy_status_ready              0x00013369   Thumb Code   100  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    drv_dsi_tx_phy_status_stopstate          0x000133d1   Thumb Code    62  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    drv_dsi_tx_phy_test_setup                0x00013415   Thumb Code   314  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    drv_dsi_tx_phy_time_cfg                  0x00013565   Thumb Code    28  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    drv_dsi_tx_powerup                       0x00013585   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    drv_dsi_tx_response_mode                 0x00013591   Thumb Code    30  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    drv_dsi_tx_set_bta_ack                   0x000135b5   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    drv_dsi_tx_set_esc_div                   0x000135d1   Thumb Code    14  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    drv_dsi_tx_set_int                       0x000135e5   Thumb Code    58  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    drv_dsi_tx_set_time_out_div              0x00013625   Thumb Code    18  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    drv_dsi_tx_set_video_chunk               0x0001363d   Thumb Code    14  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    drv_dsi_tx_set_video_timing              0x00013651   Thumb Code    30  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    drv_dsi_tx_shutdown                      0x00013675   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    drv_dsi_tx_timeout_cfg                   0x00013681   Thumb Code    38  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    drv_dsi_tx_video_mode_cfg                0x000136ad   Thumb Code   226  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    drv_efuse_enter_inactive                 0x00013795   Thumb Code    54  drv_efuse.o(i.drv_efuse_enter_inactive)
    drv_efuse_int_enable                     0x000137cb   Thumb Code    12  drv_efuse.o(i.drv_efuse_int_enable)
    drv_efuse_read                           0x000137d7   Thumb Code    58  drv_efuse.o(i.drv_efuse_read)
    drv_efuse_read_req                       0x00013811   Thumb Code    24  drv_efuse.o(i.drv_efuse_read_req)
    drv_gpio_get_attribute                   0x00013829   Thumb Code    12  drv_gpio.o(i.drv_gpio_get_attribute)
    drv_gpio_register_ap_reset_callback      0x0001385d   Thumb Code     6  drv_gpio.o(i.drv_gpio_register_ap_reset_callback)
    drv_gpio_register_callback               0x00013869   Thumb Code    14  drv_gpio.o(i.drv_gpio_register_callback)
    drv_gpio_set_attribute                   0x0001387d   Thumb Code    22  drv_gpio.o(i.drv_gpio_set_attribute)
    drv_gpio_set_int                         0x00013899   Thumb Code    62  drv_gpio.o(i.drv_gpio_set_int)
    drv_gpio_set_ioe                         0x000138dd   Thumb Code    26  drv_gpio.o(i.drv_gpio_set_ioe)
    drv_gpio_set_mode                        0x000138fd   Thumb Code    16  drv_gpio.o(i.drv_gpio_set_mode)
    drv_lcdc_bcsa_config                     0x00013931   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_bcsa_config)
    drv_lcdc_cfg_int_frame                   0x00013959   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_cfg_int_frame)
    drv_lcdc_cmd_start                       0x0001399d   Thumb Code    46  drv_lcdc.o(i.drv_lcdc_cmd_start)
    drv_lcdc_config_acc_command_mode         0x000139d1   Thumb Code    14  drv_lcdc.o(i.drv_lcdc_config_acc_command_mode)
    drv_lcdc_config_int                      0x000139e5   Thumb Code    50  drv_lcdc.o(i.drv_lcdc_config_int)
    drv_lcdc_config_int_single               0x00013a1d   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_int_single)
    drv_lcdc_config_overwrite_rgb            0x00013a45   Thumb Code    18  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    drv_lcdc_config_src_parameter            0x00013a5d   Thumb Code    72  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    drv_lcdc_crop_hact                       0x00013aad   Thumb Code    10  drv_lcdc.o(i.drv_lcdc_crop_hact)
    drv_lcdc_ctrl_flow                       0x00013abd   Thumb Code    50  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    drv_lcdc_dith_config                     0x00013af5   Thumb Code    40  drv_lcdc.o(i.drv_lcdc_dith_config)
    drv_lcdc_edge_dect_config                0x00013b25   Thumb Code    50  drv_lcdc.o(i.drv_lcdc_edge_dect_config)
    drv_lcdc_edge_enh_config                 0x00013b61   Thumb Code    86  drv_lcdc.o(i.drv_lcdc_edge_enh_config)
    drv_lcdc_enable_shadow_reg               0x00013bc5   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    drv_lcdc_endianness_config               0x00013be9   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_endianness_config)
    drv_lcdc_fc_config                       0x00013c05   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_fc_config)
    drv_lcdc_fldc_config                     0x00013c25   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_fldc_config)
    drv_lcdc_function_disable                0x00013c49   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_function_disable)
    drv_lcdc_function_enable                 0x00013c6d   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_function_enable)
    drv_lcdc_set_int                         0x00013c91   Thumb Code    54  drv_lcdc.o(i.drv_lcdc_set_int)
    drv_lcdc_set_prefetch                    0x00013ccd   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_set_prefetch)
    drv_lcdc_set_tear_line                   0x00013ce9   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_set_tear_line)
    drv_lcdc_stop_display                    0x00013d05   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_stop_display)
    drv_lcdc_vid_hw_start                    0x00013d15   Thumb Code    56  drv_lcdc.o(i.drv_lcdc_vid_hw_start)
    drv_lcdc_vintp_mode_config               0x00013d51   Thumb Code    18  drv_lcdc.o(i.drv_lcdc_vintp_mode_config)
    drv_memc_clear_status                    0x00013d69   Thumb Code    14  drv_memc.o(i.drv_memc_clear_status)
    drv_memc_enable_irq                      0x00013d7d   Thumb Code    58  drv_memc.o(i.drv_memc_enable_irq)
    drv_memc_gen_a_tear_signal               0x00013dbd   Thumb Code    12  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    drv_memc_get_status                      0x00013dcd   Thumb Code    20  drv_memc.o(i.drv_memc_get_status)
    drv_memc_get_tear_mode                   0x00013de5   Thumb Code    10  drv_memc.o(i.drv_memc_get_tear_mode)
    drv_memc_rate_transfer_sel               0x00013df5   Thumb Code    22  drv_memc.o(i.drv_memc_rate_transfer_sel)
    drv_memc_sel_vsync                       0x00013e11   Thumb Code    16  drv_memc.o(i.drv_memc_sel_vsync)
    drv_memc_set_active_height               0x00013e25   Thumb Code    16  drv_memc.o(i.drv_memc_set_active_height)
    drv_memc_set_circ_mode_enable            0x00013e3d   Thumb Code    24  drv_memc.o(i.drv_memc_set_circ_mode_enable)
    drv_memc_set_data_mode                   0x00013e59   Thumb Code    14  drv_memc.o(i.drv_memc_set_data_mode)
    drv_memc_set_double_buffer               0x00013e6d   Thumb Code    18  drv_memc.o(i.drv_memc_set_double_buffer)
    drv_memc_set_frame_drop_select           0x00013e85   Thumb Code    24  drv_memc.o(i.drv_memc_set_frame_drop_select)
    drv_memc_set_fs_en_conditions            0x00013ea1   Thumb Code    18  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    drv_memc_set_lcdc_st_conditions          0x00013eb9   Thumb Code    20  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    drv_memc_set_ltpo_mode                   0x00013ed5   Thumb Code    28  drv_memc.o(i.drv_memc_set_ltpo_mode)
    drv_memc_set_ltpo_pu_thres               0x00013ef5   Thumb Code    18  drv_memc.o(i.drv_memc_set_ltpo_pu_thres)
    drv_memc_set_tear_mode                   0x00013f0d   Thumb Code    16  drv_memc.o(i.drv_memc_set_tear_mode)
    drv_memc_set_tear_waveform               0x00013f21   Thumb Code    36  drv_memc.o(i.drv_memc_set_tear_waveform)
    drv_memc_set_vidc_sync_cnt               0x00013f4d   Thumb Code    16  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    drv_phy_test_clear                       0x00013f61   Thumb Code    16  drv_phy_common.o(i.drv_phy_test_clear)
    drv_phy_test_lock                        0x00013f71   Thumb Code    24  drv_phy_common.o(i.drv_phy_test_lock)
    drv_pwr_efuse_pd                         0x00013f89   Thumb Code    36  drv_pwr.o(i.drv_pwr_efuse_pd)
    drv_pwr_enter_deep_sleep_mode            0x00013fb9   Thumb Code    60  drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode)
    drv_pwr_enter_sleep_mode_ex              0x00014005   Thumb Code    34  drv_pwr.o(i.drv_pwr_enter_sleep_mode_ex)
    drv_pwr_enter_stop_sleep_mode            0x00014039   Thumb Code   132  drv_pwr.o(i.drv_pwr_enter_stop_sleep_mode)
    drv_pwr_exit_sleep_mode                  0x000140d1   Thumb Code    32  drv_pwr.o(i.drv_pwr_exit_sleep_mode)
    drv_pwr_get_power_ready_st               0x000140f9   Thumb Code    10  drv_pwr.o(i.drv_pwr_get_power_ready_st)
    drv_pwr_set_breath_screen_power_sel      0x00014109   Thumb Code    34  drv_pwr.o(i.drv_pwr_set_breath_screen_power_sel)
    drv_pwr_set_digit_power_sel              0x00014131   Thumb Code    34  drv_pwr.o(i.drv_pwr_set_digit_power_sel)
    drv_pwr_set_pll_clk                      0x00014159   Thumb Code    30  drv_pwr.o(i.drv_pwr_set_pll_clk)
    drv_pwr_set_wakeup_type                  0x0001418d   Thumb Code    40  drv_pwr.o(i.drv_pwr_set_wakeup_type)
    drv_pwr_write_lock                       0x000141b9   Thumb Code    18  drv_pwr.o(i.drv_pwr_write_lock)
    drv_rxbr_clear_pkt_buffer                0x000141d9   Thumb Code    12  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    drv_rxbr_clear_status0                   0x000141e9   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_clear_status0)
    drv_rxbr_enable_irq                      0x000141f5   Thumb Code    90  drv_rxbr.o(i.drv_rxbr_enable_irq)
    drv_rxbr_frame_drop_cfg                  0x00014251   Thumb Code    18  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    drv_rxbr_hline_rcv1_cfg                  0x0001429d   Thumb Code    14  drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg)
    drv_rxbr_hline_rcv_cfg                   0x000142b1   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    drv_rxbr_register_irq1_callback          0x000142c1   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    drv_rxbr_set_ack_pkt_header              0x000142cd   Thumb Code    18  drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header)
    drv_rxbr_set_color_format                0x000142e5   Thumb Code    24  drv_rxbr.o(i.drv_rxbr_set_color_format)
    drv_rxbr_set_filter_regs                 0x00014301   Thumb Code    32  drv_rxbr.o(i.drv_rxbr_set_filter_regs)
    drv_rxbr_set_inten                       0x00014325   Thumb Code    22  drv_rxbr.o(i.drv_rxbr_set_inten)
    drv_rxbr_set_ltpo_drop_th                0x00014341   Thumb Code    18  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    drv_rxbr_set_usr_cfg                     0x00014359   Thumb Code    56  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    drv_rxbr_set_usr_col                     0x00014399   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    drv_rxbr_set_usr_row                     0x000143a9   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    drv_se_init                              0x000143b9   Thumb Code   106  drv_se.o(i.drv_se_init)
    drv_se_set_dsc                           0x00014431   Thumb Code   162  drv_se.o(i.drv_se_set_dsc)
    drv_se_set_lcdc                          0x00014505   Thumb Code    88  drv_se.o(i.drv_se_set_lcdc)
    drv_se_set_memc                          0x0001458d   Thumb Code    96  drv_se.o(i.drv_se_set_memc)
    drv_se_set_rxbr                          0x0001461d   Thumb Code   158  drv_se.o(i.drv_se_set_rxbr)
    drv_se_set_vidc                          0x000146ed   Thumb Code   122  drv_se.o(i.drv_se_set_vidc)
    drv_se_start_rx                          0x00014799   Thumb Code    16  drv_se.o(i.drv_se_start_rx)
    drv_swire_enable                         0x000147ad   Thumb Code    24  drv_swire.o(i.drv_swire_enable)
    drv_swire_get_pulse_count                0x000147c9   Thumb Code     6  drv_swire.o(i.drv_swire_get_pulse_count)
    drv_swire_register_callback              0x000147d5   Thumb Code     6  drv_swire.o(i.drv_swire_register_callback)
    drv_swire_set_bit_time                   0x000147e1   Thumb Code    18  drv_swire.o(i.drv_swire_set_bit_time)
    drv_swire_set_int                        0x000147f9   Thumb Code    64  drv_swire.o(i.drv_swire_set_int)
    drv_swire_set_power_down                 0x00014841   Thumb Code    24  drv_swire.o(i.drv_swire_set_power_down)
    drv_swire_set_pulse_count                0x0001485d   Thumb Code     6  drv_swire.o(i.drv_swire_set_pulse_count)
    drv_swire_set_trig_mode                  0x00014869   Thumb Code    24  drv_swire.o(i.drv_swire_set_trig_mode)
    drv_sys_cfg_clear_all_int                0x00014885   Thumb Code     8  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    drv_sys_cfg_clear_pending                0x00014891   Thumb Code    32  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    drv_sys_cfg_sel_ap_rst_trig              0x000148b9   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig)
    drv_sys_cfg_sel_gpio_group               0x000148dd   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group)
    drv_sys_cfg_sel_int_trig                 0x00014901   Thumb Code    32  drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig)
    drv_sys_cfg_sel_swire_timer              0x00014925   Thumb Code    18  drv_sys_cfg.o(i.drv_sys_cfg_sel_swire_timer)
    drv_sys_cfg_set_int                      0x0001493d   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    drv_timer_enable                         0x0001497b   Thumb Code    32  drv_timer.o(i.drv_timer_enable)
    drv_timer_get_instance                   0x0001499d   Thumb Code    10  drv_timer.o(i.drv_timer_get_instance)
    drv_timer_set_compare_val                0x000149e9   Thumb Code    50  drv_timer.o(i.drv_timer_set_compare_val)
    drv_timer_set_int                        0x00014a29   Thumb Code    68  drv_timer.o(i.drv_timer_set_int)
    drv_timer_set_prescaler                  0x00014a71   Thumb Code    36  drv_timer.o(i.drv_timer_set_prescaler)
    drv_timer_set_repeat                     0x00014a99   Thumb Code    12  drv_timer.o(i.drv_timer_set_repeat)
    drv_tx_phy_test_enter                    0x00014aa9   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    drv_tx_phy_test_exit                     0x00014ac9   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    drv_tx_phy_test_write_code               0x00014ae9   Thumb Code    34  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    drv_uart_abort_recv                      0x00014b11   Thumb Code    46  drv_uart.o(i.drv_uart_abort_recv)
    drv_uart_abort_send                      0x00014b45   Thumb Code    46  drv_uart.o(i.drv_uart_abort_send)
    drv_uart_config_int                      0x00014b79   Thumb Code    20  drv_uart.o(i.drv_uart_config_int)
    drv_uart_enable_int                      0x00014ba5   Thumb Code    84  drv_uart.o(i.drv_uart_enable_int)
    drv_uart_get_instance                    0x00014c01   Thumb Code    36  drv_uart.o(i.drv_uart_get_instance)
    drv_uart_init                            0x00014c29   Thumb Code   206  drv_uart.o(i.drv_uart_init)
    drv_uart_reset_rx_fifo                   0x00014d35   Thumb Code    28  drv_uart.o(i.drv_uart_reset_rx_fifo)
    drv_uart_reset_tx_fifo                   0x00014d51   Thumb Code    28  drv_uart.o(i.drv_uart_reset_tx_fifo)
    drv_uart_send_blocking                   0x00014d6d   Thumb Code    26  drv_uart.o(i.drv_uart_send_blocking)
    drv_uart_set_baud_rate                   0x00014d87   Thumb Code    84  drv_uart.o(i.drv_uart_set_baud_rate)
    drv_uart_trans_create_handle             0x00014ddd   Thumb Code    72  drv_uart.o(i.drv_uart_trans_create_handle)
    drv_vidc_clear_irq                       0x00014e29   Thumb Code    10  drv_vidc.o(i.drv_vidc_clear_irq)
    drv_vidc_enable                          0x00014e39   Thumb Code    26  drv_vidc.o(i.drv_vidc_enable)
    drv_vidc_enable_irq                      0x00014e59   Thumb Code    58  drv_vidc.o(i.drv_vidc_enable_irq)
    drv_vidc_get_int_source                  0x00014e99   Thumb Code    40  drv_vidc.o(i.drv_vidc_get_int_source)
    drv_vidc_get_irq_status                  0x00014ec5   Thumb Code    20  drv_vidc.o(i.drv_vidc_get_irq_status)
    drv_vidc_init_module_enable              0x00014edd   Thumb Code    36  drv_vidc.o(i.drv_vidc_init_module_enable)
    drv_vidc_register_callback               0x00014f09   Thumb Code     6  drv_vidc.o(i.drv_vidc_register_callback)
    drv_vidc_reset                           0x00014f15   Thumb Code     8  drv_vidc.o(i.drv_vidc_reset)
    drv_vidc_set_circ_mode_enable            0x00014f21   Thumb Code    24  drv_vidc.o(i.drv_vidc_set_circ_mode_enable)
    drv_vidc_set_dither_config               0x00014f3d   Thumb Code    50  drv_vidc.o(i.drv_vidc_set_dither_config)
    drv_vidc_set_dst_parameter               0x00014f75   Thumb Code    86  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    drv_vidc_set_honly_hcoef0                0x00014fd1   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_honly_hcoef0)
    drv_vidc_set_honly_hinitb                0x00014fdd   Thumb Code    38  drv_vidc.o(i.drv_vidc_set_honly_hinitb)
    drv_vidc_set_honly_hinitr                0x00015009   Thumb Code    42  drv_vidc.o(i.drv_vidc_set_honly_hinitr)
    drv_vidc_set_irqen                       0x00015039   Thumb Code    22  drv_vidc.o(i.drv_vidc_set_irqen)
    drv_vidc_set_mirror                      0x00015055   Thumb Code    16  drv_vidc.o(i.drv_vidc_set_mirror)
    drv_vidc_set_pentile_swap                0x00015069   Thumb Code    20  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    drv_vidc_set_pu_ctrl                     0x00015085   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    drv_vidc_set_rotation                    0x00015091   Thumb Code    18  drv_vidc.o(i.drv_vidc_set_rotation)
    drv_vidc_set_scld_hcoef0                 0x000150a9   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    drv_vidc_set_scld_hcoef1                 0x000150b5   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    drv_vidc_set_scld_step                   0x000150c1   Thumb Code    14  drv_vidc.o(i.drv_vidc_set_scld_step)
    drv_vidc_set_scld_vcoef0                 0x000150d5   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    drv_vidc_set_scld_vcoef1                 0x000150e1   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    drv_vidc_set_src_parameter               0x000150ed   Thumb Code    28  drv_vidc.o(i.drv_vidc_set_src_parameter)
    drv_vidc_set_vintp_config                0x0001510d   Thumb Code    52  drv_vidc.o(i.drv_vidc_set_vintp_config)
    fputc                                    0x00015145   Thumb Code    42  tau_log.o(i.fputc)
    google_p6a_demo                          0x00015179   Thumb Code    54  p6a_demo.o(i.google_p6a_demo)
    hal_dsi_rx_ctrl_create_handle            0x00015221   Thumb Code    60  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    hal_dsi_rx_ctrl_dcs_async_handler        0x00015261   Thumb Code    60  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler)
    hal_dsi_rx_ctrl_deinit                   0x000152a1   Thumb Code   132  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit)
    hal_dsi_rx_ctrl_get_max_ret_size         0x00015335   Thumb Code    28  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size)
    hal_dsi_rx_ctrl_init                     0x00015355   Thumb Code   158  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    hal_dsi_rx_ctrl_pre_init_pps             0x00015aed   Thumb Code    50  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    hal_dsi_rx_ctrl_send_ack_cmd             0x00015b25   Thumb Code   210  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd)
    hal_dsi_rx_ctrl_start                    0x00015c45   Thumb Code    42  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    hal_dsi_rx_ctrl_stop                     0x00015c75   Thumb Code    42  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop)
    hal_dsi_rx_ctrl_toggle_resolution        0x00015ca5   Thumb Code    28  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    hal_dsi_tx_ctrl_create_handle            0x00015f41   Thumb Code    48  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    hal_dsi_tx_ctrl_deinit                   0x00015f79   Thumb Code   102  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit)
    hal_dsi_tx_ctrl_gen_a_tear_signal        0x00015fed   Thumb Code    34  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal)
    hal_dsi_tx_ctrl_init                     0x00016011   Thumb Code   110  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    hal_dsi_tx_ctrl_set_overwrite_rgb        0x0001609d   Thumb Code     8  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    hal_dsi_tx_ctrl_set_tear_mode            0x000160a5   Thumb Code    10  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode)
    hal_dsi_tx_ctrl_start                    0x000160b1   Thumb Code   116  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    hal_dsi_tx_ctrl_stop                     0x0001612d   Thumb Code    52  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop)
    hal_dsi_tx_ctrl_write_array_cmd          0x00016165   Thumb Code   238  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd)
    hal_dsi_tx_ctrl_write_cmd                0x00016259   Thumb Code   202  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    hal_gpio_config_pad                      0x0001690d   Thumb Code    58  hal_gpio.o(i.hal_gpio_config_pad)
    hal_gpio_ctrl_eint                       0x00016949   Thumb Code    18  hal_gpio.o(i.hal_gpio_ctrl_eint)
    hal_gpio_init_eint                       0x00016961   Thumb Code    58  hal_gpio.o(i.hal_gpio_init_eint)
    hal_gpio_init_input                      0x000169a1   Thumb Code    22  hal_gpio.o(i.hal_gpio_init_input)
    hal_gpio_init_output                     0x000169b7   Thumb Code    28  hal_gpio.o(i.hal_gpio_init_output)
    hal_gpio_reg_eint_cb                     0x000169d5   Thumb Code    22  hal_gpio.o(i.hal_gpio_reg_eint_cb)
    hal_gpio_set_ap_reset_int                0x000169f1   Thumb Code    76  hal_gpio.o(i.hal_gpio_set_ap_reset_int)
    hal_gpio_set_high_impedance              0x00016a41   Thumb Code    32  hal_gpio.o(i.hal_gpio_set_high_impedance)
    hal_gpio_set_mode                        0x00016a61   Thumb Code    94  hal_gpio.o(i.hal_gpio_set_mode)
    hal_gpio_set_output_data                 0x00016ac5   Thumb Code     8  hal_gpio.o(i.hal_gpio_set_output_data)
    hal_gpio_set_pull_state                  0x00016acd   Thumb Code    66  hal_gpio.o(i.hal_gpio_set_pull_state)
    hal_internal_sync_get_hight_performan_mode 0x00016b15   Thumb Code    10  hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode)
    hal_internal_sync_input_resolution_change 0x00016b25   Thumb Code   330  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    hal_internal_sync_register_lcdc_cb       0x00016cd9   Thumb Code     8  hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb)
    hal_internal_vsync_deinit                0x00016ce5   Thumb Code    22  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    hal_internal_vsync_get_rx_state          0x00016d05   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state)
    hal_internal_vsync_get_sync_line         0x00016d11   Thumb Code    16  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    hal_internal_vsync_get_tx_state          0x00016d25   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    hal_internal_vsync_init_rx               0x00016d31   Thumb Code   190  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    hal_internal_vsync_init_tx               0x00016e09   Thumb Code   194  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    hal_internal_vsync_set_rx_state          0x00016ed1   Thumb Code    28  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    hal_internal_vsync_set_tear_mode         0x00016ef1   Thumb Code   262  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    hal_internal_vsync_set_tx_state          0x00017009   Thumb Code    92  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    hal_intl_dcs_init_sw_fltr                0x00017075   Thumb Code    90  hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr)
    hal_intl_dcs_set_auto_hw_filter          0x00017729   Thumb Code   130  hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter)
    hal_intl_fb_cal_fb_info                  0x000177e1   Thumb Code   738  hal_internal_fb.o(i.hal_intl_fb_cal_fb_info)
    hal_intl_fb_get_memc_flow_mode           0x00017c75   Thumb Code     6  hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode)
    hal_intl_fb_get_rx_fb_info               0x00017c81   Thumb Code    12  hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info)
    hal_intl_fb_get_tx_fb_info               0x00017c91   Thumb Code    12  hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info)
    hal_intl_fb_get_user_flow                0x00017ca1   Thumb Code     6  hal_internal_fb.o(i.hal_intl_fb_get_user_flow)
    hal_intl_svs_deinit_rx                   0x00017cad   Thumb Code    32  hal_internal_svs.o(i.hal_intl_svs_deinit_rx)
    hal_intl_svs_deinit_tx                   0x00017cd5   Thumb Code    10  hal_internal_svs.o(i.hal_intl_svs_deinit_tx)
    hal_intl_svs_handle                      0x00017ce5   Thumb Code    24  hal_internal_svs.o(i.hal_intl_svs_handle)
    hal_intl_svs_init_rx                     0x00017d09   Thumb Code   120  hal_internal_svs.o(i.hal_intl_svs_init_rx)
    hal_intl_svs_init_tx                     0x00017d89   Thumb Code    16  hal_internal_svs.o(i.hal_intl_svs_init_tx)
    hal_intl_svs_set_rx_vtt                  0x00017d9d   Thumb Code     6  hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt)
    hal_intl_svs_update_rxbr_clk             0x00017da9   Thumb Code    52  hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk)
    hal_lcdc_displayproc_config              0x00017df1   Thumb Code    94  hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config)
    hal_lcdc_postproc_config                 0x00017f11   Thumb Code   276  hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config)
    hal_lcdc_upscaler_config                 0x00018099   Thumb Code   202  hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config)
    hal_nonshadow_func_update                0x00018179   Thumb Code   180  hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update)
    hal_pwr_enter_deep_sleep_mode            0x00018235   Thumb Code    42  hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode)
    hal_pwr_enter_normal_sleep_mode          0x0001825f   Thumb Code     8  hal_pwr.o(i.hal_pwr_enter_normal_sleep_mode)
    hal_pwr_enter_stop_sleep_mode            0x00018269   Thumb Code    88  hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode)
    hal_pwr_exit_sleep_mode                  0x000182cd   Thumb Code    10  hal_pwr.o(i.hal_pwr_exit_sleep_mode)
    hal_pwr_get_vcc_power_ready              0x000182d7   Thumb Code     8  hal_pwr.o(i.hal_pwr_get_vcc_power_ready)
    hal_pwr_set_main_power                   0x000182df   Thumb Code     8  hal_pwr.o(i.hal_pwr_set_main_power)
    hal_pwr_set_sleep_mode_power             0x000182e7   Thumb Code     8  hal_pwr.o(i.hal_pwr_set_sleep_mode_power)
    hal_pwr_set_stop_sleep_wakeup_pin        0x000182f1   Thumb Code    86  hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin)
    hal_swire_deinit                         0x00018355   Thumb Code    60  hal_swire.o(i.hal_swire_deinit)
    hal_swire_enable                         0x00018395   Thumb Code    86  hal_swire.o(i.hal_swire_enable)
    hal_swire_init                           0x000183f1   Thumb Code    74  hal_swire.o(i.hal_swire_init)
    hal_swire_set_pulse                      0x00018449   Thumb Code    32  hal_swire.o(i.hal_swire_set_pulse)
    hal_swire_set_timer                      0x0001846d   Thumb Code    60  hal_swire.o(i.hal_swire_set_timer)
    hal_system_init                          0x000184ad   Thumb Code   192  hal_system.o(i.hal_system_init)
    hal_system_updata_sysclk                 0x00018591   Thumb Code    60  hal_system.o(i.hal_system_updata_sysclk)
    hal_timer_deinit                         0x000185e1   Thumb Code    48  hal_timer.o(i.hal_timer_deinit)
    hal_timer_init                           0x00018611   Thumb Code    28  hal_timer.o(i.hal_timer_init)
    hal_timer_set_repeat                     0x0001862d   Thumb Code     8  hal_timer.o(i.hal_timer_set_repeat)
    hal_uart_init                            0x00018665   Thumb Code   134  hal_uart.o(i.hal_uart_init)
    hal_uart_send_blocking                   0x000186f9   Thumb Code    24  hal_uart.o(i.hal_uart_send_blocking)
    hal_vsync_func_update                    0x00018715   Thumb Code    18  hal_dsi_tx_ctrl.o(i.hal_vsync_func_update)
    hal_vsync_reset_lcdc_scaler              0x0001872d   Thumb Code   188  hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler)
    main                                     0x000187f9   Thumb Code    32  main.o(i.main)
    tau_log_init                             0x00019065   Thumb Code    48  tau_log.o(i.tau_log_init)
    tau_log_printf                           0x00019099   Thumb Code   116  tau_log.o(i.tau_log_printf)
    tau_log_push_log                         0x0001911d   Thumb Code   118  tau_log.o(i.tau_log_push_log)
    panel_init_code                          0x000193c0   Data        8250  p6a_demo.o(.constdata)
    Region$$Table$$Base                      0x0001b644   Number         0  anon$$obj.o(Region$$Table)
    Region$$Table$$Limit                     0x0001b664   Number         0  anon$$obj.o(Region$$Table)
    rd_51_val                                0x00070018   Data           2  p6a_demo.o(.data)
    rd_51_val2                               0x0007001a   Data           2  p6a_demo.o(.data)
    pps                                      0x0007001c   Data         128  p6a_demo.o(.data)
    pps_fhd                                  0x0007009c   Data         128  p6a_demo.o(.data)
    value_51H                                0x0007011c   Data           1  p6a_demo.o(.data)
    value_51L                                0x0007011d   Data           1  p6a_demo.o(.data)
    sg_uart0_tx_handle                       0x000701b0   Data           4  hal_uart.o(.data)
    sg_uart0_rx_handle                       0x000701b4   Data           4  hal_uart.o(.data)
    sg_uart1_tx_handle                       0x000701b8   Data           4  hal_uart.o(.data)
    sg_uart1_rx_handle                       0x000701bc   Data           4  hal_uart.o(.data)
    g_sof_gen_te_func                        0x000701cc   Data           4  hal_internal_vsync.o(.data)
    hal_internal_vsync_handle_callback       0x000701d0   Data           4  hal_internal_vsync.o(.data)
    hal_internal_disp_end_handle_callback    0x000701d4   Data           4  hal_internal_vsync.o(.data)
    g_systick_cb_func                        0x00070204   Data           4  drv_common.o(.data)
    g_system_clock                           0x00070208   Data           4  drv_common.o(.data)
    g_system_delay_step                      0x0007020c   Data           1  drv_common.o(.data)
    g_int_rxbr_irq0_cb_func                  0x00070270   Data           4  drv_rxbr.o(.data)
    g_int_rxbr_irq1_cb_func                  0x00070274   Data           4  drv_rxbr.o(.data)
    g_int_vidc_cb_func                       0x00070278   Data           4  drv_vidc.o(.data)
    dma_req_map                              0x0007037c   Data         144  drv_dma.o(.data)
    __stdout                                 0x0007040c   Data           4  stdout.o(.data)
    g_vsync_handle                           0x00070698   Data          40  hal_internal_vsync.o(.bss)
    g_dcs_execute_table                      0x000706c0   Data        2048  hal_internal_dcs.o(.bss)
    g_rx_fb_info                             0x00070fc0   Data          68  hal_internal_fb.o(.bss)
    g_packet_fifo                            0x00071088   Data        4204  dcs_packet_fifo.o(.bss)
    __stack_limit                            0x00072168   Data           0  startup_armcm0.o(STACK)
    __initial_sp                             0x00073168   Data           0  startup_armcm0.o(STACK)



==============================================================================

Memory Map of the image

  Image Entry point : 0x000100c1

  Load Region LR_IROM2 (Base: 0x00010000, Size: 0x0000ba74, Max: 0x00010000, ABSOLUTE, COMPRESSED[0x0000b7d0])

    Execution Region ER_IROM2 (Exec base: 0x00010000, Load base: 0x00010000, Size: 0x0000b664, Max: 0x00010000, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00010000   0x00010000   0x000000c0   Data   RO          323    RESET               startup_armcm0.o
    0x000100c0   0x000100c0   0x00000000   Code   RO         1866  * .ARM.Collect$$$$00000000  mc_p.l(entry.o)
    0x000100c0   0x000100c0   0x00000004   Code   RO         2170    .ARM.Collect$$$$00000001  mc_p.l(entry2.o)
    0x000100c4   0x000100c4   0x00000004   Code   RO         2173    .ARM.Collect$$$$00000004  mc_p.l(entry5.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         2175    .ARM.Collect$$$$00000008  mc_p.l(entry7b.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         2177    .ARM.Collect$$$$0000000A  mc_p.l(entry8b.o)
    0x000100c8   0x000100c8   0x00000008   Code   RO         2178    .ARM.Collect$$$$0000000B  mc_p.l(entry9a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         2180    .ARM.Collect$$$$0000000D  mc_p.l(entry10a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         2182    .ARM.Collect$$$$0000000F  mc_p.l(entry11a.o)
    0x000100d0   0x000100d0   0x00000004   Code   RO         2171    .ARM.Collect$$$$00002712  mc_p.l(entry2.o)
    0x000100d4   0x000100d4   0x00000078   Code   RO          324    .text               startup_armcm0.o
    0x0001014c   0x0001014c   0x0000002c   Code   RO         1869    .text               mc_p.l(uidiv.o)
    0x00010178   0x00010178   0x00000028   Code   RO         1871    .text               mc_p.l(idiv.o)
    0x000101a0   0x000101a0   0x00000024   Code   RO         1873    .text               mc_p.l(memcpya.o)
    0x000101c4   0x000101c4   0x00000024   Code   RO         1875    .text               mc_p.l(memseta.o)
    0x000101e8   0x000101e8   0x0000000e   Code   RO         1877    .text               mc_p.l(strlen.o)
    0x000101f6   0x000101f6   0x000000b2   Code   RO         2142    .text               mf_p.l(fadd.o)
    0x000102a8   0x000102a8   0x0000007a   Code   RO         2144    .text               mf_p.l(fmul.o)
    0x00010322   0x00010322   0x0000007c   Code   RO         2146    .text               mf_p.l(fdiv.o)
    0x0001039e   0x0001039e   0x00000018   Code   RO         2148    .text               mf_p.l(fscalb.o)
    0x000103b6   0x000103b6   0x00000002   PAD
    0x000103b8   0x000103b8   0x00000164   Code   RO         2150    .text               mf_p.l(dadd.o)
    0x0001051c   0x0001051c   0x000000d0   Code   RO         2152    .text               mf_p.l(dmul.o)
    0x000105ec   0x000105ec   0x0000000e   Code   RO         2154    .text               mf_p.l(ffltui.o)
    0x000105fa   0x000105fa   0x00000002   PAD
    0x000105fc   0x000105fc   0x0000001c   Code   RO         2156    .text               mf_p.l(dfltui.o)
    0x00010618   0x00010618   0x00000028   Code   RO         2158    .text               mf_p.l(ffixui.o)
    0x00010640   0x00010640   0x0000003c   Code   RO         2160    .text               mf_p.l(dfixui.o)
    0x0001067c   0x0001067c   0x00000028   Code   RO         2162    .text               mf_p.l(f2d.o)
    0x000106a4   0x000106a4   0x00000038   Code   RO         2164    .text               mf_p.l(d2f.o)
    0x000106dc   0x000106dc   0x00000014   Code   RO         2166    .text               mf_p.l(cfcmple.o)
    0x000106f0   0x000106f0   0x00000014   Code   RO         2168    .text               mf_p.l(cfrcmple.o)
    0x00010704   0x00010704   0x00000060   Code   RO         2185    .text               mc_p.l(uldiv.o)
    0x00010764   0x00010764   0x00000020   Code   RO         2187    .text               mc_p.l(llshl.o)
    0x00010784   0x00010784   0x00000022   Code   RO         2189    .text               mc_p.l(llushr.o)
    0x000107a6   0x000107a6   0x00000026   Code   RO         2191    .text               mc_p.l(llsshr.o)
    0x000107cc   0x000107cc   0x00000000   Code   RO         2193    .text               mc_p.l(iusefp.o)
    0x000107cc   0x000107cc   0x00000082   Code   RO         2194    .text               mf_p.l(fepilogue.o)
    0x0001084e   0x0001084e   0x000000be   Code   RO         2196    .text               mf_p.l(depilogue.o)
    0x0001090c   0x0001090c   0x000000f0   Code   RO         2200    .text               mf_p.l(ddiv.o)
    0x000109fc   0x000109fc   0x00000040   Code   RO         2202    .text               mf_p.l(dfixul.o)
    0x00010a3c   0x00010a3c   0x00000028   Code   RO         2204    .text               mf_p.l(cdrcmple.o)
    0x00010a64   0x00010a64   0x00000024   Code   RO         2206    .text               mc_p.l(init.o)
    0x00010a88   0x00010a88   0x00000056   Code   RO         2216    .text               mc_p.l(__dczerorl2.o)
    0x00010ade   0x00010ade   0x00000002   PAD
    0x00010ae0   0x00010ae0   0x0000001c   Code   RO          948    i.AP_NRESET_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010afc   0x00010afc   0x0000005c   Code   RO         1715    i.DMA_IRQn_Handler  CVWL668T.lib(drv_dma.o)
    0x00010b58   0x00010b58   0x0000000a   Code   RO          949    i.EXTI_INT0_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010b62   0x00010b62   0x0000000a   Code   RO          950    i.EXTI_INT1_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010b6c   0x00010b6c   0x0000000a   Code   RO          951    i.EXTI_INT2_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010b76   0x00010b76   0x0000000a   Code   RO          952    i.EXTI_INT3_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010b80   0x00010b80   0x0000000a   Code   RO          953    i.EXTI_INT4_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010b8a   0x00010b8a   0x0000000a   Code   RO          954    i.EXTI_INT5_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010b94   0x00010b94   0x0000000a   Code   RO          955    i.EXTI_INT6_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010b9e   0x00010b9e   0x0000000a   Code   RO          956    i.EXTI_INT7_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010ba8   0x00010ba8   0x00000048   Code   RO          871    i.HardFault_Handler  CVWL668T.lib(drv_common.o)
    0x00010bf0   0x00010bf0   0x00000100   Code   RO          720    i.LCDC_IRQn_Handler  CVWL668T.lib(hal_internal_vsync.o)
    0x00010cf0   0x00010cf0   0x0000009a   Code   RO         1475    i.MEMC_IRQn_Handler  CVWL668T.lib(drv_memc.o)
    0x00010d8a   0x00010d8a   0x00000002   PAD
    0x00010d8c   0x00010d8c   0x000000b8   Code   RO         1281    i.MIPI_TX_IRQn_Handler  CVWL668T.lib(drv_dsi_tx.o)
    0x00010e44   0x00010e44   0x00000030   Code   RO         1110    i.SWIRE_IRQn_Handler  CVWL668T.lib(drv_swire.o)
    0x00010e74   0x00010e74   0x00000018   Code   RO          872    i.SysTick_Handler   CVWL668T.lib(drv_common.o)
    0x00010e8c   0x00010e8c   0x0000000a   Code   RO         1153    i.TIMER0_IRQn_Handler  CVWL668T.lib(drv_timer.o)
    0x00010e96   0x00010e96   0x0000000a   Code   RO         1154    i.TIMER1_IRQn_Handler  CVWL668T.lib(drv_timer.o)
    0x00010ea0   0x00010ea0   0x0000000a   Code   RO         1155    i.TIMER2_IRQn_Handler  CVWL668T.lib(drv_timer.o)
    0x00010eaa   0x00010eaa   0x0000000a   Code   RO         1156    i.TIMER3_IRQn_Handler  CVWL668T.lib(drv_timer.o)
    0x00010eb4   0x00010eb4   0x0000001c   Code   RO         1630    i.VIDC_IRQn_Handler  CVWL668T.lib(drv_vidc.o)
    0x00010ed0   0x00010ed0   0x0000001c   Code   RO         1541    i.VPRE1_IRQn_Handler  CVWL668T.lib(drv_rxbr.o)
    0x00010eec   0x00010eec   0x0000007c   Code   RO          782    i.VPRE_IRQn_Handler  CVWL668T.lib(hal_internal_dcs.o)
    0x00010f68   0x00010f68   0x00000020   Code   RO         2114    i.__0printf         mc_p.l(printfa.o)
    0x00010f88   0x00010f88   0x00000024   Code   RO         2120    i.__0vsprintf       mc_p.l(printfa.o)
    0x00010fac   0x00010fac   0x0000002e   Code   RO         2198    i.__ARM_clz         mf_p.l(depilogue.o)
    0x00010fda   0x00010fda   0x0000001a   Code   RO          408    i.__ARM_common_switch8  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00010ff4   0x00010ff4   0x00000002   Code   RO         2211    i.__scatterload_null  mc_p.l(handlers.o)
    0x00010ff6   0x00010ff6   0x0000000a   Code   RO         2126    i._sputc            mc_p.l(printfa.o)
    0x00011000   0x00011000   0x0000001c   Data   RO          879    .ARM.__at_0x11000   CVWL668T.lib(drv_common.o)
    0x0001101c   0x0001101c   0x00000010   Data   RO          676    .ARM.__at_0x1101C   CVWL668T.lib(tau_log.o)
    0x0001102c   0x0001102c   0x00000016   Data   RO          461    .ARM.__at_0x1102C   CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00011042   0x00011042   0x00000002   PAD
    0x00011044   0x00011044   0x00000364   Code   RO         1220    i.MIPI_RX_IRQn_Handler  CVWL668T.lib(drv_dsi_rx.o)
    0x000113a8   0x000113a8   0x00000180   Code   RO         1778    i.UART_IRQn_Handler  CVWL668T.lib(drv_uart.o)
    0x00011528   0x00011528   0x00000020   Code   RO         1542    i.__NVIC_DisableIRQ  CVWL668T.lib(drv_rxbr.o)
    0x00011548   0x00011548   0x00000018   Code   RO         1543    i.__NVIC_EnableIRQ  CVWL668T.lib(drv_rxbr.o)
    0x00011560   0x00011560   0x0000000e   Code   RO         2210    i.__scatterload_copy  mc_p.l(handlers.o)
    0x0001156e   0x0001156e   0x0000000e   Code   RO         2212    i.__scatterload_zeroinit  mc_p.l(handlers.o)
    0x0001157c   0x0001157c   0x00000174   Code   RO         2121    i._fp_digits        mc_p.l(printfa.o)
    0x000116f0   0x000116f0   0x000006ec   Code   RO         2122    i._printf_core      mc_p.l(printfa.o)
    0x00011ddc   0x00011ddc   0x00000020   Code   RO         2123    i._printf_post_padding  mc_p.l(printfa.o)
    0x00011dfc   0x00011dfc   0x0000002c   Code   RO         2124    i._printf_pre_padding  mc_p.l(printfa.o)
    0x00011e28   0x00011e28   0x00000144   Code   RO           95    i.ap_dcs_read       p6a_demo.o
    0x00011f6c   0x00011f6c   0x000000a4   Code   RO           96    i.ap_dcs_set_backlight  p6a_demo.o
    0x00012010   0x00012010   0x00000058   Code   RO           97    i.ap_dcs_set_display_off  p6a_demo.o
    0x00012068   0x00012068   0x000000a0   Code   RO           98    i.ap_dcs_set_display_on  p6a_demo.o
    0x00012108   0x00012108   0x00000088   Code   RO           99    i.ap_dcs_set_enter_sleep_mode  p6a_demo.o
    0x00012190   0x00012190   0x00000040   Code   RO          101    i.ap_dcs_set_exit_sleep_mode  p6a_demo.o
    0x000121d0   0x000121d0   0x00000034   Code   RO          102    i.ap_dcs_set_frame_change  p6a_demo.o
    0x00012204   0x00012204   0x00000058   Code   RO          103    i.ap_rstn_pull_down_cb  p6a_demo.o
    0x0001225c   0x0001225c   0x0000001c   Code   RO          104    i.ap_rstn_pull_high_cb  p6a_demo.o
    0x00012278   0x00012278   0x0000004a   Code   RO          105    i.ap_set_FPS_B1     p6a_demo.o
    0x000122c2   0x000122c2   0x0000002c   Code   RO          106    i.app_display_init  p6a_demo.o
    0x000122ee   0x000122ee   0x00000002   PAD
    0x000122f0   0x000122f0   0x0000001c   Code   RO          107    i.app_gpio_init     p6a_demo.o
    0x0001230c   0x0001230c   0x00000034   Code   RO          108    i.app_init_panel    p6a_demo.o
    0x00012340   0x00012340   0x00000120   Code   RO          109    i.app_mipi_rx_init  p6a_demo.o
    0x00012460   0x00012460   0x000000fc   Code   RO          110    i.app_mipi_tx_init  p6a_demo.o
    0x0001255c   0x0001255c   0x000000a8   Code   RO          111    i.app_mipi_tx_start  p6a_demo.o
    0x00012604   0x00012604   0x0000006c   Code   RO          112    i.app_system_process  p6a_demo.o
    0x00012670   0x00012670   0x00000044   Code   RO          113    i.app_system_resume  p6a_demo.o
    0x000126b4   0x000126b4   0x00000190   Code   RO          114    i.app_system_suspend  p6a_demo.o
    0x00012844   0x00012844   0x0000002e   Code   RO          115    i.app_tx_panel_reset  p6a_demo.o
    0x00012872   0x00012872   0x00000002   PAD
    0x00012874   0x00012874   0x00000018   Code   RO          297    i.board_Init        board.o
    0x0001288c   0x0001288c   0x000000c8   Code   RO         1863    i.ceil              m_ps.l(ceil.o)
    0x00012954   0x00012954   0x0000002c   Code   RO          721    i.check_mipi_rx_tx_video_info  CVWL668T.lib(hal_internal_vsync.o)
    0x00012980   0x00012980   0x00000088   Code   RO          783    i.check_pkt_buf_rev  CVWL668T.lib(hal_internal_dcs.o)
    0x00012a08   0x00012a08   0x00000058   Code   RO         1186    i.dcs_packet_fifo_alloc  CVWL668T.lib(dcs_packet_fifo.o)
    0x00012a60   0x00012a60   0x00000018   Code   RO         1187    i.dcs_packet_fifo_init  CVWL668T.lib(dcs_packet_fifo.o)
    0x00012a78   0x00012a78   0x00000044   Code   RO         1188    i.dcs_packet_free_fifo_header  CVWL668T.lib(dcs_packet_fifo.o)
    0x00012abc   0x00012abc   0x00000024   Code   RO         1189    i.dcs_packet_get_fifo_header  CVWL668T.lib(dcs_packet_fifo.o)
    0x00012ae0   0x00012ae0   0x00000018   Code   RO          663    i.delayMs           CVWL668T.lib(tau_delay.o)
    0x00012af8   0x00012af8   0x0000002c   Code   RO          664    i.delayUs           CVWL668T.lib(tau_delay.o)
    0x00012b24   0x00012b24   0x00000008   Code   RO          877    i.drv_common_system_init  CVWL668T.lib(drv_common.o)
    0x00012b2c   0x00012b2c   0x0000003c   Code   RO          896    i.drv_crgu_enable_clock  CVWL668T.lib(drv_crgu.o)
    0x00012b68   0x00012b68   0x00000068   Code   RO          899    i.drv_crgu_get_rxbr_clk  CVWL668T.lib(drv_crgu.o)
    0x00012bd0   0x00012bd0   0x00000010   Code   RO          902    i.drv_crgu_reset_modules  CVWL668T.lib(drv_crgu.o)
    0x00012be0   0x00012be0   0x00000028   Code   RO          903    i.drv_crgu_set_ahb_clk  CVWL668T.lib(drv_crgu.o)
    0x00012c08   0x00012c08   0x00000010   Code   RO          904    i.drv_crgu_set_clock_div  CVWL668T.lib(drv_crgu.o)
    0x00012c18   0x00012c18   0x0000003c   Code   RO          906    i.drv_crgu_set_dpi_clk  CVWL668T.lib(drv_crgu.o)
    0x00012c54   0x00012c54   0x00000038   Code   RO          907    i.drv_crgu_set_dsc_clk  CVWL668T.lib(drv_crgu.o)
    0x00012c8c   0x00012c8c   0x00000028   Code   RO          908    i.drv_crgu_set_fb_clk  CVWL668T.lib(drv_crgu.o)
    0x00012cb4   0x00012cb4   0x00000028   Code   RO          909    i.drv_crgu_set_lcdc_clk  CVWL668T.lib(drv_crgu.o)
    0x00012cdc   0x00012cdc   0x00000018   Code   RO          910    i.drv_crgu_set_reset  CVWL668T.lib(drv_crgu.o)
    0x00012cf4   0x00012cf4   0x00000028   Code   RO          911    i.drv_crgu_set_rxbr_clk  CVWL668T.lib(drv_crgu.o)
    0x00012d1c   0x00012d1c   0x00000028   Code   RO          912    i.drv_crgu_set_vidc_clk  CVWL668T.lib(drv_crgu.o)
    0x00012d44   0x00012d44   0x00000018   Code   RO         1717    i.drv_dma_clear_status  CVWL668T.lib(drv_dma.o)
    0x00012d5c   0x00012d5c   0x00000014   Code   RO         1723    i.drv_dma_get_int_source  CVWL668T.lib(drv_dma.o)
    0x00012d70   0x00012d70   0x0000001c   Code   RO          936    i.drv_dsc_dec_disable  CVWL668T.lib(drv_dsc_dec.o)
    0x00012d8c   0x00012d8c   0x00000038   Code   RO          937    i.drv_dsc_dec_enable  CVWL668T.lib(drv_dsc_dec.o)
    0x00012dc4   0x00012dc4   0x00000020   Code   RO          938    i.drv_dsc_dec_get_nslc  CVWL668T.lib(drv_dsc_dec.o)
    0x00012de4   0x00012de4   0x0000001c   Code   RO          939    i.drv_dsc_dec_set_irqen  CVWL668T.lib(drv_dsc_dec.o)
    0x00012e00   0x00012e00   0x0000010c   Code   RO         1221    i.drv_dsi_rx_calc_ipi_tx_delay  CVWL668T.lib(drv_dsi_rx.o)
    0x00012f0c   0x00012f0c   0x00000040   Code   RO         1222    i.drv_dsi_rx_enable_irq  CVWL668T.lib(drv_dsi_rx.o)
    0x00012f4c   0x00012f4c   0x00000050   Code   RO         1224    i.drv_dsi_rx_get_color_bpp  CVWL668T.lib(drv_dsi_rx.o)
    0x00012f9c   0x00012f9c   0x0000001c   Code   RO         1225    i.drv_dsi_rx_get_color_pcc  CVWL668T.lib(drv_dsi_rx.o)
    0x00012fb8   0x00012fb8   0x00000010   Code   RO         1226    i.drv_dsi_rx_get_compression_en  CVWL668T.lib(drv_dsi_rx.o)
    0x00012fc8   0x00012fc8   0x00000010   Code   RO         1227    i.drv_dsi_rx_get_ddi_crc_en  CVWL668T.lib(drv_dsi_rx.o)
    0x00012fd8   0x00012fd8   0x0000000c   Code   RO         1229    i.drv_dsi_rx_get_max_ret_size  CVWL668T.lib(drv_dsi_rx.o)
    0x00012fe4   0x00012fe4   0x00000018   Code   RO         1232    i.drv_dsi_rx_power_up  CVWL668T.lib(drv_dsi_rx.o)
    0x00012ffc   0x00012ffc   0x0000001c   Code   RO         1233    i.drv_dsi_rx_set_check_crc  CVWL668T.lib(drv_dsi_rx.o)
    0x00013018   0x00013018   0x00000024   Code   RO         1234    i.drv_dsi_rx_set_ctrl_cfg  CVWL668T.lib(drv_dsi_rx.o)
    0x0001303c   0x0001303c   0x00000010   Code   RO         1235    i.drv_dsi_rx_set_ddi_cfg  CVWL668T.lib(drv_dsi_rx.o)
    0x0001304c   0x0001304c   0x0000001c   Code   RO         1236    i.drv_dsi_rx_set_ddi_crc_en  CVWL668T.lib(drv_dsi_rx.o)
    0x00013068   0x00013068   0x0000000c   Code   RO         1239    i.drv_dsi_rx_set_inten  CVWL668T.lib(drv_dsi_rx.o)
    0x00013074   0x00013074   0x00000010   Code   RO         1240    i.drv_dsi_rx_set_ipi_cfg  CVWL668T.lib(drv_dsi_rx.o)
    0x00013084   0x00013084   0x0000001c   Code   RO         1242    i.drv_dsi_rx_set_ipi_ycbcr_frmt  CVWL668T.lib(drv_dsi_rx.o)
    0x000130a0   0x000130a0   0x00000014   Code   RO         1243    i.drv_dsi_rx_set_lane_swap  CVWL668T.lib(drv_dsi_rx.o)
    0x000130b4   0x000130b4   0x00000024   Code   RO         1244    i.drv_dsi_rx_set_resp_cnt  CVWL668T.lib(drv_dsi_rx.o)
    0x000130d8   0x000130d8   0x0000001c   Code   RO         1245    i.drv_dsi_rx_set_tear_resp_en  CVWL668T.lib(drv_dsi_rx.o)
    0x000130f4   0x000130f4   0x00000100   Code   RO         1246    i.drv_dsi_rx_set_up_phy  CVWL668T.lib(drv_dsi_rx.o)
    0x000131f4   0x000131f4   0x00000018   Code   RO         1247    i.drv_dsi_rx_shut_down  CVWL668T.lib(drv_dsi_rx.o)
    0x0001320c   0x0001320c   0x00000018   Code   RO         1283    i.drv_dsi_tx_command_header  CVWL668T.lib(drv_dsi_tx.o)
    0x00013224   0x00013224   0x00000058   Code   RO         1284    i.drv_dsi_tx_command_mode_cfg  CVWL668T.lib(drv_dsi_tx.o)
    0x0001327c   0x0001327c   0x0000000c   Code   RO         1285    i.drv_dsi_tx_command_put_payload  CVWL668T.lib(drv_dsi_tx.o)
    0x00013288   0x00013288   0x00000020   Code   RO         1286    i.drv_dsi_tx_config_eotp  CVWL668T.lib(drv_dsi_tx.o)
    0x000132a8   0x000132a8   0x0000000c   Code   RO         1287    i.drv_dsi_tx_config_int  CVWL668T.lib(drv_dsi_tx.o)
    0x000132b4   0x000132b4   0x00000010   Code   RO         1288    i.drv_dsi_tx_dpi_lpcmd_time  CVWL668T.lib(drv_dsi_tx.o)
    0x000132c4   0x000132c4   0x00000010   Code   RO         1289    i.drv_dsi_tx_dpi_mode  CVWL668T.lib(drv_dsi_tx.o)
    0x000132d4   0x000132d4   0x00000024   Code   RO         1290    i.drv_dsi_tx_dpi_polarity  CVWL668T.lib(drv_dsi_tx.o)
    0x000132f8   0x000132f8   0x0000000c   Code   RO         1291    i.drv_dsi_tx_edpi_cmd_size  CVWL668T.lib(drv_dsi_tx.o)
    0x00013304   0x00013304   0x0000000c   Code   RO         1293    i.drv_dsi_tx_get_cmd_status  CVWL668T.lib(drv_dsi_tx.o)
    0x00013310   0x00013310   0x0000000c   Code   RO         1295    i.drv_dsi_tx_mode   CVWL668T.lib(drv_dsi_tx.o)
    0x0001331c   0x0001331c   0x0000001c   Code   RO         1296    i.drv_dsi_tx_phy_clock_lane_auto_lp  CVWL668T.lib(drv_dsi_tx.o)
    0x00013338   0x00013338   0x00000020   Code   RO         1297    i.drv_dsi_tx_phy_clock_lane_req_hs  CVWL668T.lib(drv_dsi_tx.o)
    0x00013358   0x00013358   0x00000010   Code   RO         1299    i.drv_dsi_tx_phy_lane_mode  CVWL668T.lib(drv_dsi_tx.o)
    0x00013368   0x00013368   0x00000068   Code   RO         1302    i.drv_dsi_tx_phy_status_ready  CVWL668T.lib(drv_dsi_tx.o)
    0x000133d0   0x000133d0   0x00000044   Code   RO         1303    i.drv_dsi_tx_phy_status_stopstate  CVWL668T.lib(drv_dsi_tx.o)
    0x00013414   0x00013414   0x00000150   Code   RO         1305    i.drv_dsi_tx_phy_test_setup  CVWL668T.lib(drv_dsi_tx.o)
    0x00013564   0x00013564   0x00000020   Code   RO         1306    i.drv_dsi_tx_phy_time_cfg  CVWL668T.lib(drv_dsi_tx.o)
    0x00013584   0x00013584   0x0000000c   Code   RO         1310    i.drv_dsi_tx_powerup  CVWL668T.lib(drv_dsi_tx.o)
    0x00013590   0x00013590   0x00000024   Code   RO         1311    i.drv_dsi_tx_response_mode  CVWL668T.lib(drv_dsi_tx.o)
    0x000135b4   0x000135b4   0x0000001c   Code   RO         1314    i.drv_dsi_tx_set_bta_ack  CVWL668T.lib(drv_dsi_tx.o)
    0x000135d0   0x000135d0   0x00000014   Code   RO         1315    i.drv_dsi_tx_set_esc_div  CVWL668T.lib(drv_dsi_tx.o)
    0x000135e4   0x000135e4   0x00000040   Code   RO         1316    i.drv_dsi_tx_set_int  CVWL668T.lib(drv_dsi_tx.o)
    0x00013624   0x00013624   0x00000018   Code   RO         1317    i.drv_dsi_tx_set_time_out_div  CVWL668T.lib(drv_dsi_tx.o)
    0x0001363c   0x0001363c   0x00000014   Code   RO         1318    i.drv_dsi_tx_set_video_chunk  CVWL668T.lib(drv_dsi_tx.o)
    0x00013650   0x00013650   0x00000024   Code   RO         1319    i.drv_dsi_tx_set_video_timing  CVWL668T.lib(drv_dsi_tx.o)
    0x00013674   0x00013674   0x0000000c   Code   RO         1321    i.drv_dsi_tx_shutdown  CVWL668T.lib(drv_dsi_tx.o)
    0x00013680   0x00013680   0x0000002c   Code   RO         1322    i.drv_dsi_tx_timeout_cfg  CVWL668T.lib(drv_dsi_tx.o)
    0x000136ac   0x000136ac   0x000000e8   Code   RO         1325    i.drv_dsi_tx_video_mode_cfg  CVWL668T.lib(drv_dsi_tx.o)
    0x00013794   0x00013794   0x00000036   Code   RO         1823    i.drv_efuse_enter_inactive  CVWL668T.lib(drv_efuse.o)
    0x000137ca   0x000137ca   0x0000000c   Code   RO         1826    i.drv_efuse_int_enable  CVWL668T.lib(drv_efuse.o)
    0x000137d6   0x000137d6   0x0000003a   Code   RO         1827    i.drv_efuse_read    CVWL668T.lib(drv_efuse.o)
    0x00013810   0x00013810   0x00000018   Code   RO         1828    i.drv_efuse_read_req  CVWL668T.lib(drv_efuse.o)
    0x00013828   0x00013828   0x00000010   Code   RO          957    i.drv_gpio_get_attribute  CVWL668T.lib(drv_gpio.o)
    0x00013838   0x00013838   0x00000024   Code   RO          959    i.drv_gpio_handle_int  CVWL668T.lib(drv_gpio.o)
    0x0001385c   0x0001385c   0x0000000c   Code   RO          960    i.drv_gpio_register_ap_reset_callback  CVWL668T.lib(drv_gpio.o)
    0x00013868   0x00013868   0x00000014   Code   RO          961    i.drv_gpio_register_callback  CVWL668T.lib(drv_gpio.o)
    0x0001387c   0x0001387c   0x0000001c   Code   RO          962    i.drv_gpio_set_attribute  CVWL668T.lib(drv_gpio.o)
    0x00013898   0x00013898   0x00000044   Code   RO          963    i.drv_gpio_set_int  CVWL668T.lib(drv_gpio.o)
    0x000138dc   0x000138dc   0x00000020   Code   RO          964    i.drv_gpio_set_ioe  CVWL668T.lib(drv_gpio.o)
    0x000138fc   0x000138fc   0x00000014   Code   RO          965    i.drv_gpio_set_mode  CVWL668T.lib(drv_gpio.o)
    0x00013910   0x00013910   0x00000020   Code   RO          518    i.drv_gpio_set_output_data  CVWL668T.lib(hal_gpio.o)
    0x00013930   0x00013930   0x00000028   Code   RO         1387    i.drv_lcdc_bcsa_config  CVWL668T.lib(drv_lcdc.o)
    0x00013958   0x00013958   0x0000002c   Code   RO         1388    i.drv_lcdc_cfg_int_frame  CVWL668T.lib(drv_lcdc.o)
    0x00013984   0x00013984   0x00000018   Code   RO         1389    i.drv_lcdc_clear_int  CVWL668T.lib(drv_lcdc.o)
    0x0001399c   0x0001399c   0x00000034   Code   RO         1391    i.drv_lcdc_cmd_start  CVWL668T.lib(drv_lcdc.o)
    0x000139d0   0x000139d0   0x00000014   Code   RO         1392    i.drv_lcdc_config_acc_command_mode  CVWL668T.lib(drv_lcdc.o)
    0x000139e4   0x000139e4   0x00000038   Code   RO         1393    i.drv_lcdc_config_int  CVWL668T.lib(drv_lcdc.o)
    0x00013a1c   0x00013a1c   0x00000028   Code   RO         1394    i.drv_lcdc_config_int_single  CVWL668T.lib(drv_lcdc.o)
    0x00013a44   0x00013a44   0x00000018   Code   RO         1395    i.drv_lcdc_config_overwrite_rgb  CVWL668T.lib(drv_lcdc.o)
    0x00013a5c   0x00013a5c   0x00000050   Code   RO         1396    i.drv_lcdc_config_src_parameter  CVWL668T.lib(drv_lcdc.o)
    0x00013aac   0x00013aac   0x00000010   Code   RO         1397    i.drv_lcdc_crop_hact  CVWL668T.lib(drv_lcdc.o)
    0x00013abc   0x00013abc   0x00000038   Code   RO         1398    i.drv_lcdc_ctrl_flow  CVWL668T.lib(drv_lcdc.o)
    0x00013af4   0x00013af4   0x00000030   Code   RO         1399    i.drv_lcdc_dith_config  CVWL668T.lib(drv_lcdc.o)
    0x00013b24   0x00013b24   0x0000003c   Code   RO         1401    i.drv_lcdc_edge_dect_config  CVWL668T.lib(drv_lcdc.o)
    0x00013b60   0x00013b60   0x00000064   Code   RO         1402    i.drv_lcdc_edge_enh_config  CVWL668T.lib(drv_lcdc.o)
    0x00013bc4   0x00013bc4   0x00000024   Code   RO         1403    i.drv_lcdc_enable_shadow_reg  CVWL668T.lib(drv_lcdc.o)
    0x00013be8   0x00013be8   0x0000001c   Code   RO         1404    i.drv_lcdc_endianness_config  CVWL668T.lib(drv_lcdc.o)
    0x00013c04   0x00013c04   0x00000020   Code   RO         1405    i.drv_lcdc_fc_config  CVWL668T.lib(drv_lcdc.o)
    0x00013c24   0x00013c24   0x00000024   Code   RO         1407    i.drv_lcdc_fldc_config  CVWL668T.lib(drv_lcdc.o)
    0x00013c48   0x00013c48   0x00000024   Code   RO         1408    i.drv_lcdc_function_disable  CVWL668T.lib(drv_lcdc.o)
    0x00013c6c   0x00013c6c   0x00000024   Code   RO         1409    i.drv_lcdc_function_enable  CVWL668T.lib(drv_lcdc.o)
    0x00013c90   0x00013c90   0x0000003c   Code   RO         1420    i.drv_lcdc_set_int  CVWL668T.lib(drv_lcdc.o)
    0x00013ccc   0x00013ccc   0x0000001c   Code   RO         1421    i.drv_lcdc_set_prefetch  CVWL668T.lib(drv_lcdc.o)
    0x00013ce8   0x00013ce8   0x0000001c   Code   RO         1422    i.drv_lcdc_set_tear_line  CVWL668T.lib(drv_lcdc.o)
    0x00013d04   0x00013d04   0x00000010   Code   RO         1424    i.drv_lcdc_stop_display  CVWL668T.lib(drv_lcdc.o)
    0x00013d14   0x00013d14   0x0000003c   Code   RO         1426    i.drv_lcdc_vid_hw_start  CVWL668T.lib(drv_lcdc.o)
    0x00013d50   0x00013d50   0x00000018   Code   RO         1428    i.drv_lcdc_vintp_mode_config  CVWL668T.lib(drv_lcdc.o)
    0x00013d68   0x00013d68   0x00000014   Code   RO         1476    i.drv_memc_clear_status  CVWL668T.lib(drv_memc.o)
    0x00013d7c   0x00013d7c   0x00000040   Code   RO         1477    i.drv_memc_enable_irq  CVWL668T.lib(drv_memc.o)
    0x00013dbc   0x00013dbc   0x00000010   Code   RO         1478    i.drv_memc_gen_a_tear_signal  CVWL668T.lib(drv_memc.o)
    0x00013dcc   0x00013dcc   0x00000018   Code   RO         1479    i.drv_memc_get_status  CVWL668T.lib(drv_memc.o)
    0x00013de4   0x00013de4   0x00000010   Code   RO         1480    i.drv_memc_get_tear_mode  CVWL668T.lib(drv_memc.o)
    0x00013df4   0x00013df4   0x0000001c   Code   RO         1481    i.drv_memc_rate_transfer_sel  CVWL668T.lib(drv_memc.o)
    0x00013e10   0x00013e10   0x00000014   Code   RO         1482    i.drv_memc_sel_vsync  CVWL668T.lib(drv_memc.o)
    0x00013e24   0x00013e24   0x00000018   Code   RO         1483    i.drv_memc_set_active_height  CVWL668T.lib(drv_memc.o)
    0x00013e3c   0x00013e3c   0x0000001c   Code   RO         1484    i.drv_memc_set_circ_mode_enable  CVWL668T.lib(drv_memc.o)
    0x00013e58   0x00013e58   0x00000014   Code   RO         1485    i.drv_memc_set_data_mode  CVWL668T.lib(drv_memc.o)
    0x00013e6c   0x00013e6c   0x00000018   Code   RO         1488    i.drv_memc_set_double_buffer  CVWL668T.lib(drv_memc.o)
    0x00013e84   0x00013e84   0x0000001c   Code   RO         1492    i.drv_memc_set_frame_drop_select  CVWL668T.lib(drv_memc.o)
    0x00013ea0   0x00013ea0   0x00000018   Code   RO         1493    i.drv_memc_set_fs_en_conditions  CVWL668T.lib(drv_memc.o)
    0x00013eb8   0x00013eb8   0x0000001c   Code   RO         1495    i.drv_memc_set_lcdc_st_conditions  CVWL668T.lib(drv_memc.o)
    0x00013ed4   0x00013ed4   0x00000020   Code   RO         1496    i.drv_memc_set_ltpo_mode  CVWL668T.lib(drv_memc.o)
    0x00013ef4   0x00013ef4   0x00000018   Code   RO         1497    i.drv_memc_set_ltpo_pu_thres  CVWL668T.lib(drv_memc.o)
    0x00013f0c   0x00013f0c   0x00000014   Code   RO         1501    i.drv_memc_set_tear_mode  CVWL668T.lib(drv_memc.o)
    0x00013f20   0x00013f20   0x0000002c   Code   RO         1502    i.drv_memc_set_tear_waveform  CVWL668T.lib(drv_memc.o)
    0x00013f4c   0x00013f4c   0x00000014   Code   RO         1504    i.drv_memc_set_vidc_sync_cnt  CVWL668T.lib(drv_memc.o)
    0x00013f60   0x00013f60   0x00000010   Code   RO         1846    i.drv_phy_test_clear  CVWL668T.lib(drv_phy_common.o)
    0x00013f70   0x00013f70   0x00000018   Code   RO         1847    i.drv_phy_test_lock  CVWL668T.lib(drv_phy_common.o)
    0x00013f88   0x00013f88   0x00000030   Code   RO          995    i.drv_pwr_efuse_pd  CVWL668T.lib(drv_pwr.o)
    0x00013fb8   0x00013fb8   0x0000004c   Code   RO          997    i.drv_pwr_enter_deep_sleep_mode  CVWL668T.lib(drv_pwr.o)
    0x00014004   0x00014004   0x00000034   Code   RO          999    i.drv_pwr_enter_sleep_mode_ex  CVWL668T.lib(drv_pwr.o)
    0x00014038   0x00014038   0x00000098   Code   RO         1000    i.drv_pwr_enter_stop_sleep_mode  CVWL668T.lib(drv_pwr.o)
    0x000140d0   0x000140d0   0x00000028   Code   RO         1001    i.drv_pwr_exit_sleep_mode  CVWL668T.lib(drv_pwr.o)
    0x000140f8   0x000140f8   0x00000010   Code   RO         1004    i.drv_pwr_get_power_ready_st  CVWL668T.lib(drv_pwr.o)
    0x00014108   0x00014108   0x00000028   Code   RO         1036    i.drv_pwr_set_breath_screen_power_sel  CVWL668T.lib(drv_pwr.o)
    0x00014130   0x00014130   0x00000028   Code   RO         1037    i.drv_pwr_set_digit_power_sel  CVWL668T.lib(drv_pwr.o)
    0x00014158   0x00014158   0x00000034   Code   RO         1040    i.drv_pwr_set_pll_clk  CVWL668T.lib(drv_pwr.o)
    0x0001418c   0x0001418c   0x0000002c   Code   RO         1044    i.drv_pwr_set_wakeup_type  CVWL668T.lib(drv_pwr.o)
    0x000141b8   0x000141b8   0x00000020   Code   RO         1047    i.drv_pwr_write_lock  CVWL668T.lib(drv_pwr.o)
    0x000141d8   0x000141d8   0x00000010   Code   RO         1544    i.drv_rxbr_clear_pkt_buffer  CVWL668T.lib(drv_rxbr.o)
    0x000141e8   0x000141e8   0x0000000c   Code   RO         1545    i.drv_rxbr_clear_status0  CVWL668T.lib(drv_rxbr.o)
    0x000141f4   0x000141f4   0x0000005a   Code   RO         1548    i.drv_rxbr_enable_irq  CVWL668T.lib(drv_rxbr.o)
    0x0001424e   0x0001424e   0x00000002   PAD
    0x00014250   0x00014250   0x0000001c   Code   RO         1549    i.drv_rxbr_frame_drop_cfg  CVWL668T.lib(drv_rxbr.o)
    0x0001426c   0x0001426c   0x00000018   Code   RO          722    i.drv_rxbr_get_int_source  CVWL668T.lib(hal_internal_vsync.o)
    0x00014284   0x00014284   0x00000018   Code   RO          784    i.drv_rxbr_get_status0  CVWL668T.lib(hal_internal_dcs.o)
    0x0001429c   0x0001429c   0x00000014   Code   RO         1559    i.drv_rxbr_hline_rcv1_cfg  CVWL668T.lib(drv_rxbr.o)
    0x000142b0   0x000142b0   0x00000010   Code   RO         1560    i.drv_rxbr_hline_rcv_cfg  CVWL668T.lib(drv_rxbr.o)
    0x000142c0   0x000142c0   0x0000000c   Code   RO         1562    i.drv_rxbr_register_irq1_callback  CVWL668T.lib(drv_rxbr.o)
    0x000142cc   0x000142cc   0x00000018   Code   RO         1563    i.drv_rxbr_set_ack_pkt_header  CVWL668T.lib(drv_rxbr.o)
    0x000142e4   0x000142e4   0x0000001c   Code   RO         1568    i.drv_rxbr_set_color_format  CVWL668T.lib(drv_rxbr.o)
    0x00014300   0x00014300   0x00000024   Code   RO         1571    i.drv_rxbr_set_filter_regs  CVWL668T.lib(drv_rxbr.o)
    0x00014324   0x00014324   0x0000001c   Code   RO         1572    i.drv_rxbr_set_inten  CVWL668T.lib(drv_rxbr.o)
    0x00014340   0x00014340   0x00000018   Code   RO         1573    i.drv_rxbr_set_ltpo_drop_th  CVWL668T.lib(drv_rxbr.o)
    0x00014358   0x00014358   0x00000040   Code   RO         1577    i.drv_rxbr_set_usr_cfg  CVWL668T.lib(drv_rxbr.o)
    0x00014398   0x00014398   0x00000010   Code   RO         1578    i.drv_rxbr_set_usr_col  CVWL668T.lib(drv_rxbr.o)
    0x000143a8   0x000143a8   0x00000010   Code   RO         1579    i.drv_rxbr_set_usr_row  CVWL668T.lib(drv_rxbr.o)
    0x000143b8   0x000143b8   0x00000078   Code   RO         1201    i.drv_se_init       CVWL668T.lib(drv_se.o)
    0x00014430   0x00014430   0x000000d4   Code   RO         1202    i.drv_se_set_dsc    CVWL668T.lib(drv_se.o)
    0x00014504   0x00014504   0x00000088   Code   RO         1203    i.drv_se_set_lcdc   CVWL668T.lib(drv_se.o)
    0x0001458c   0x0001458c   0x00000090   Code   RO         1204    i.drv_se_set_memc   CVWL668T.lib(drv_se.o)
    0x0001461c   0x0001461c   0x000000d0   Code   RO         1205    i.drv_se_set_rxbr   CVWL668T.lib(drv_se.o)
    0x000146ec   0x000146ec   0x000000ac   Code   RO         1206    i.drv_se_set_vidc   CVWL668T.lib(drv_se.o)
    0x00014798   0x00014798   0x00000014   Code   RO         1207    i.drv_se_start_rx   CVWL668T.lib(drv_se.o)
    0x000147ac   0x000147ac   0x0000001c   Code   RO         1111    i.drv_swire_enable  CVWL668T.lib(drv_swire.o)
    0x000147c8   0x000147c8   0x0000000c   Code   RO         1112    i.drv_swire_get_pulse_count  CVWL668T.lib(drv_swire.o)
    0x000147d4   0x000147d4   0x0000000c   Code   RO         1113    i.drv_swire_register_callback  CVWL668T.lib(drv_swire.o)
    0x000147e0   0x000147e0   0x00000018   Code   RO         1114    i.drv_swire_set_bit_time  CVWL668T.lib(drv_swire.o)
    0x000147f8   0x000147f8   0x00000048   Code   RO         1115    i.drv_swire_set_int  CVWL668T.lib(drv_swire.o)
    0x00014840   0x00014840   0x0000001c   Code   RO         1116    i.drv_swire_set_power_down  CVWL668T.lib(drv_swire.o)
    0x0001485c   0x0001485c   0x0000000c   Code   RO         1117    i.drv_swire_set_pulse_count  CVWL668T.lib(drv_swire.o)
    0x00014868   0x00014868   0x0000001c   Code   RO         1118    i.drv_swire_set_trig_mode  CVWL668T.lib(drv_swire.o)
    0x00014884   0x00014884   0x0000000c   Code   RO         1133    i.drv_sys_cfg_clear_all_int  CVWL668T.lib(drv_sys_cfg.o)
    0x00014890   0x00014890   0x00000028   Code   RO         1134    i.drv_sys_cfg_clear_pending  CVWL668T.lib(drv_sys_cfg.o)
    0x000148b8   0x000148b8   0x00000024   Code   RO         1135    i.drv_sys_cfg_sel_ap_rst_trig  CVWL668T.lib(drv_sys_cfg.o)
    0x000148dc   0x000148dc   0x00000024   Code   RO         1137    i.drv_sys_cfg_sel_gpio_group  CVWL668T.lib(drv_sys_cfg.o)
    0x00014900   0x00014900   0x00000024   Code   RO         1138    i.drv_sys_cfg_sel_int_trig  CVWL668T.lib(drv_sys_cfg.o)
    0x00014924   0x00014924   0x00000018   Code   RO         1139    i.drv_sys_cfg_sel_swire_timer  CVWL668T.lib(drv_sys_cfg.o)
    0x0001493c   0x0001493c   0x00000024   Code   RO         1140    i.drv_sys_cfg_set_int  CVWL668T.lib(drv_sys_cfg.o)
    0x00014960   0x00014960   0x0000001a   Code   RO         1157    i.drv_timer_clear_status_flags  CVWL668T.lib(drv_timer.o)
    0x0001497a   0x0001497a   0x00000020   Code   RO         1158    i.drv_timer_enable  CVWL668T.lib(drv_timer.o)
    0x0001499a   0x0001499a   0x00000002   PAD
    0x0001499c   0x0001499c   0x00000010   Code   RO         1159    i.drv_timer_get_instance  CVWL668T.lib(drv_timer.o)
    0x000149ac   0x000149ac   0x0000003c   Code   RO         1161    i.drv_timer_handle_interrupt  CVWL668T.lib(drv_timer.o)
    0x000149e8   0x000149e8   0x00000040   Code   RO         1163    i.drv_timer_set_compare_val  CVWL668T.lib(drv_timer.o)
    0x00014a28   0x00014a28   0x00000048   Code   RO         1164    i.drv_timer_set_int  CVWL668T.lib(drv_timer.o)
    0x00014a70   0x00014a70   0x00000028   Code   RO         1165    i.drv_timer_set_prescaler  CVWL668T.lib(drv_timer.o)
    0x00014a98   0x00014a98   0x00000010   Code   RO         1166    i.drv_timer_set_repeat  CVWL668T.lib(drv_timer.o)
    0x00014aa8   0x00014aa8   0x00000020   Code   RO         1327    i.drv_tx_phy_test_enter  CVWL668T.lib(drv_dsi_tx.o)
    0x00014ac8   0x00014ac8   0x00000020   Code   RO         1328    i.drv_tx_phy_test_exit  CVWL668T.lib(drv_dsi_tx.o)
    0x00014ae8   0x00014ae8   0x00000028   Code   RO         1331    i.drv_tx_phy_test_write_code  CVWL668T.lib(drv_dsi_tx.o)
    0x00014b10   0x00014b10   0x00000034   Code   RO         1779    i.drv_uart_abort_recv  CVWL668T.lib(drv_uart.o)
    0x00014b44   0x00014b44   0x00000034   Code   RO         1780    i.drv_uart_abort_send  CVWL668T.lib(drv_uart.o)
    0x00014b78   0x00014b78   0x00000014   Code   RO         1781    i.drv_uart_config_int  CVWL668T.lib(drv_uart.o)
    0x00014b8c   0x00014b8c   0x00000018   Code   RO         1783    i.drv_uart_enable_clk  CVWL668T.lib(drv_uart.o)
    0x00014ba4   0x00014ba4   0x0000005c   Code   RO         1784    i.drv_uart_enable_int  CVWL668T.lib(drv_uart.o)
    0x00014c00   0x00014c00   0x00000028   Code   RO         1786    i.drv_uart_get_instance  CVWL668T.lib(drv_uart.o)
    0x00014c28   0x00014c28   0x000000ce   Code   RO         1787    i.drv_uart_init     CVWL668T.lib(drv_uart.o)
    0x00014cf6   0x00014cf6   0x00000002   PAD
    0x00014cf8   0x00014cf8   0x0000003c   Code   RO         1788    i.drv_uart_int_trans_handle  CVWL668T.lib(drv_uart.o)
    0x00014d34   0x00014d34   0x0000001c   Code   RO         1791    i.drv_uart_reset_rx_fifo  CVWL668T.lib(drv_uart.o)
    0x00014d50   0x00014d50   0x0000001c   Code   RO         1792    i.drv_uart_reset_tx_fifo  CVWL668T.lib(drv_uart.o)
    0x00014d6c   0x00014d6c   0x0000001a   Code   RO         1793    i.drv_uart_send_blocking  CVWL668T.lib(drv_uart.o)
    0x00014d86   0x00014d86   0x00000054   Code   RO         1795    i.drv_uart_set_baud_rate  CVWL668T.lib(drv_uart.o)
    0x00014dda   0x00014dda   0x00000002   PAD
    0x00014ddc   0x00014ddc   0x0000004c   Code   RO         1796    i.drv_uart_trans_create_handle  CVWL668T.lib(drv_uart.o)
    0x00014e28   0x00014e28   0x00000010   Code   RO         1631    i.drv_vidc_clear_irq  CVWL668T.lib(drv_vidc.o)
    0x00014e38   0x00014e38   0x00000020   Code   RO         1635    i.drv_vidc_enable   CVWL668T.lib(drv_vidc.o)
    0x00014e58   0x00014e58   0x00000040   Code   RO         1636    i.drv_vidc_enable_irq  CVWL668T.lib(drv_vidc.o)
    0x00014e98   0x00014e98   0x0000002c   Code   RO         1637    i.drv_vidc_get_int_source  CVWL668T.lib(drv_vidc.o)
    0x00014ec4   0x00014ec4   0x00000018   Code   RO         1638    i.drv_vidc_get_irq_status  CVWL668T.lib(drv_vidc.o)
    0x00014edc   0x00014edc   0x0000002c   Code   RO         1642    i.drv_vidc_init_module_enable  CVWL668T.lib(drv_vidc.o)
    0x00014f08   0x00014f08   0x0000000c   Code   RO         1643    i.drv_vidc_register_callback  CVWL668T.lib(drv_vidc.o)
    0x00014f14   0x00014f14   0x0000000c   Code   RO         1644    i.drv_vidc_reset    CVWL668T.lib(drv_vidc.o)
    0x00014f20   0x00014f20   0x0000001c   Code   RO         1645    i.drv_vidc_set_circ_mode_enable  CVWL668T.lib(drv_vidc.o)
    0x00014f3c   0x00014f3c   0x00000038   Code   RO         1646    i.drv_vidc_set_dither_config  CVWL668T.lib(drv_vidc.o)
    0x00014f74   0x00014f74   0x0000005c   Code   RO         1648    i.drv_vidc_set_dst_parameter  CVWL668T.lib(drv_vidc.o)
    0x00014fd0   0x00014fd0   0x0000000c   Code   RO         1650    i.drv_vidc_set_honly_hcoef0  CVWL668T.lib(drv_vidc.o)
    0x00014fdc   0x00014fdc   0x0000002c   Code   RO         1651    i.drv_vidc_set_honly_hinitb  CVWL668T.lib(drv_vidc.o)
    0x00015008   0x00015008   0x00000030   Code   RO         1652    i.drv_vidc_set_honly_hinitr  CVWL668T.lib(drv_vidc.o)
    0x00015038   0x00015038   0x0000001c   Code   RO         1655    i.drv_vidc_set_irqen  CVWL668T.lib(drv_vidc.o)
    0x00015054   0x00015054   0x00000014   Code   RO         1656    i.drv_vidc_set_mirror  CVWL668T.lib(drv_vidc.o)
    0x00015068   0x00015068   0x0000001c   Code   RO         1659    i.drv_vidc_set_pentile_swap  CVWL668T.lib(drv_vidc.o)
    0x00015084   0x00015084   0x0000000c   Code   RO         1660    i.drv_vidc_set_pu_ctrl  CVWL668T.lib(drv_vidc.o)
    0x00015090   0x00015090   0x00000018   Code   RO         1661    i.drv_vidc_set_rotation  CVWL668T.lib(drv_vidc.o)
    0x000150a8   0x000150a8   0x0000000c   Code   RO         1662    i.drv_vidc_set_scld_hcoef0  CVWL668T.lib(drv_vidc.o)
    0x000150b4   0x000150b4   0x0000000c   Code   RO         1663    i.drv_vidc_set_scld_hcoef1  CVWL668T.lib(drv_vidc.o)
    0x000150c0   0x000150c0   0x00000014   Code   RO         1664    i.drv_vidc_set_scld_step  CVWL668T.lib(drv_vidc.o)
    0x000150d4   0x000150d4   0x0000000c   Code   RO         1665    i.drv_vidc_set_scld_vcoef0  CVWL668T.lib(drv_vidc.o)
    0x000150e0   0x000150e0   0x0000000c   Code   RO         1666    i.drv_vidc_set_scld_vcoef1  CVWL668T.lib(drv_vidc.o)
    0x000150ec   0x000150ec   0x00000020   Code   RO         1667    i.drv_vidc_set_src_parameter  CVWL668T.lib(drv_vidc.o)
    0x0001510c   0x0001510c   0x00000038   Code   RO         1668    i.drv_vidc_set_vintp_config  CVWL668T.lib(drv_vidc.o)
    0x00015144   0x00015144   0x00000034   Code   RO          672    i.fputc             CVWL668T.lib(tau_log.o)
    0x00015178   0x00015178   0x00000068   Code   RO          116    i.google_p6a_demo   p6a_demo.o
    0x000151e0   0x000151e0   0x00000040   Code   RO          812    i.ha_intl_fb_check_pu_size  CVWL668T.lib(hal_internal_fb.o)
    0x00015220   0x00015220   0x00000040   Code   RO          332    i.hal_dsi_rx_ctrl_create_handle  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00015260   0x00015260   0x00000040   Code   RO          333    i.hal_dsi_rx_ctrl_dcs_async_handler  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x000152a0   0x000152a0   0x00000094   Code   RO          334    i.hal_dsi_rx_ctrl_deinit  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00015334   0x00015334   0x00000020   Code   RO          339    i.hal_dsi_rx_ctrl_get_max_ret_size  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00015354   0x00015354   0x000000ac   Code   RO          340    i.hal_dsi_rx_ctrl_init  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00015400   0x00015400   0x00000100   Code   RO          341    i.hal_dsi_rx_ctrl_init_clk  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00015500   0x00015500   0x000000f8   Code   RO          342    i.hal_dsi_rx_ctrl_init_dsi_rx  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x000155f8   0x000155f8   0x0000012c   Code   RO          343    i.hal_dsi_rx_ctrl_init_memc  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00015724   0x00015724   0x00000148   Code   RO          344    i.hal_dsi_rx_ctrl_init_rxbr  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x0001586c   0x0001586c   0x00000280   Code   RO          345    i.hal_dsi_rx_ctrl_init_vidc  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00015aec   0x00015aec   0x00000038   Code   RO          346    i.hal_dsi_rx_ctrl_pre_init_pps  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00015b24   0x00015b24   0x000000f0   Code   RO          351    i.hal_dsi_rx_ctrl_send_ack_cmd  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00015c14   0x00015c14   0x00000030   Code   RO          357    i.hal_dsi_rx_ctrl_set_ipi_cfg  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00015c44   0x00015c44   0x00000030   Code   RO          362    i.hal_dsi_rx_ctrl_start  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00015c74   0x00015c74   0x00000030   Code   RO          363    i.hal_dsi_rx_ctrl_stop  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00015ca4   0x00015ca4   0x00000020   Code   RO          365    i.hal_dsi_rx_ctrl_toggle_resolution  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00015cc4   0x00015cc4   0x0000027c   Code   RO          412    i.hal_dsi_tx_cmd_mode_cal_timing  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00015f40   0x00015f40   0x00000038   Code   RO          414    i.hal_dsi_tx_ctrl_create_handle  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00015f78   0x00015f78   0x00000074   Code   RO          415    i.hal_dsi_tx_ctrl_deinit  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00015fec   0x00015fec   0x00000022   Code   RO          418    i.hal_dsi_tx_ctrl_gen_a_tear_signal  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001600e   0x0001600e   0x00000002   PAD
    0x00016010   0x00016010   0x0000007c   Code   RO          420    i.hal_dsi_tx_ctrl_init  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001608c   0x0001608c   0x00000010   Code   RO          421    i.hal_dsi_tx_ctrl_init_clk  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001609c   0x0001609c   0x00000008   Code   RO          434    i.hal_dsi_tx_ctrl_set_overwrite_rgb  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x000160a4   0x000160a4   0x0000000a   Code   RO          435    i.hal_dsi_tx_ctrl_set_tear_mode  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x000160ae   0x000160ae   0x00000002   PAD
    0x000160b0   0x000160b0   0x0000007c   Code   RO          437    i.hal_dsi_tx_ctrl_start  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001612c   0x0001612c   0x00000038   Code   RO          438    i.hal_dsi_tx_ctrl_stop  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00016164   0x00016164   0x000000f4   Code   RO          440    i.hal_dsi_tx_ctrl_write_array_cmd  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00016258   0x00016258   0x000000d0   Code   RO          441    i.hal_dsi_tx_ctrl_write_cmd  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00016328   0x00016328   0x0000010c   Code   RO          442    i.hal_dsi_tx_init_cfg  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00016434   0x00016434   0x00000038   Code   RO          443    i.hal_dsi_tx_init_dpi_timing  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001646c   0x0001646c   0x00000016   Code   RO          444    i.hal_dsi_tx_init_phy_cfg  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00016482   0x00016482   0x00000052   Code   RO          445    i.hal_dsi_tx_init_timing  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x000164d4   0x000164d4   0x00000054   Code   RO          446    i.hal_dsi_tx_init_vid_timing  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00016528   0x00016528   0x00000040   Code   RO          447    i.hal_dsi_tx_send_cmd  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00016568   0x00016568   0x00000094   Code   RO          448    i.hal_dsi_tx_timing_info_update  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x000165fc   0x000165fc   0x00000310   Code   RO          449    i.hal_dsi_tx_vid_mode_cal_timing  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001690c   0x0001690c   0x0000003a   Code   RO          519    i.hal_gpio_config_pad  CVWL668T.lib(hal_gpio.o)
    0x00016946   0x00016946   0x00000002   PAD
    0x00016948   0x00016948   0x00000018   Code   RO          520    i.hal_gpio_ctrl_eint  CVWL668T.lib(hal_gpio.o)
    0x00016960   0x00016960   0x00000040   Code   RO          524    i.hal_gpio_init_eint  CVWL668T.lib(hal_gpio.o)
    0x000169a0   0x000169a0   0x00000016   Code   RO          525    i.hal_gpio_init_input  CVWL668T.lib(hal_gpio.o)
    0x000169b6   0x000169b6   0x0000001c   Code   RO          526    i.hal_gpio_init_output  CVWL668T.lib(hal_gpio.o)
    0x000169d2   0x000169d2   0x00000002   PAD
    0x000169d4   0x000169d4   0x0000001c   Code   RO          527    i.hal_gpio_reg_eint_cb  CVWL668T.lib(hal_gpio.o)
    0x000169f0   0x000169f0   0x00000050   Code   RO          528    i.hal_gpio_set_ap_reset_int  CVWL668T.lib(hal_gpio.o)
    0x00016a40   0x00016a40   0x00000020   Code   RO          530    i.hal_gpio_set_high_impedance  CVWL668T.lib(hal_gpio.o)
    0x00016a60   0x00016a60   0x00000064   Code   RO          531    i.hal_gpio_set_mode  CVWL668T.lib(hal_gpio.o)
    0x00016ac4   0x00016ac4   0x00000008   Code   RO          532    i.hal_gpio_set_output_data  CVWL668T.lib(hal_gpio.o)
    0x00016acc   0x00016acc   0x00000048   Code   RO          533    i.hal_gpio_set_pull_state  CVWL668T.lib(hal_gpio.o)
    0x00016b14   0x00016b14   0x00000010   Code   RO          724    i.hal_internal_sync_get_hight_performan_mode  CVWL668T.lib(hal_internal_vsync.o)
    0x00016b24   0x00016b24   0x000001b4   Code   RO          725    i.hal_internal_sync_input_resolution_change  CVWL668T.lib(hal_internal_vsync.o)
    0x00016cd8   0x00016cd8   0x0000000c   Code   RO          726    i.hal_internal_sync_register_lcdc_cb  CVWL668T.lib(hal_internal_vsync.o)
    0x00016ce4   0x00016ce4   0x00000020   Code   RO          729    i.hal_internal_vsync_deinit  CVWL668T.lib(hal_internal_vsync.o)
    0x00016d04   0x00016d04   0x0000000c   Code   RO          730    i.hal_internal_vsync_get_rx_state  CVWL668T.lib(hal_internal_vsync.o)
    0x00016d10   0x00016d10   0x00000014   Code   RO          731    i.hal_internal_vsync_get_sync_line  CVWL668T.lib(hal_internal_vsync.o)
    0x00016d24   0x00016d24   0x0000000c   Code   RO          732    i.hal_internal_vsync_get_tx_state  CVWL668T.lib(hal_internal_vsync.o)
    0x00016d30   0x00016d30   0x000000d8   Code   RO          733    i.hal_internal_vsync_init_rx  CVWL668T.lib(hal_internal_vsync.o)
    0x00016e08   0x00016e08   0x000000c8   Code   RO          734    i.hal_internal_vsync_init_tx  CVWL668T.lib(hal_internal_vsync.o)
    0x00016ed0   0x00016ed0   0x00000020   Code   RO          735    i.hal_internal_vsync_set_rx_state  CVWL668T.lib(hal_internal_vsync.o)
    0x00016ef0   0x00016ef0   0x00000118   Code   RO          737    i.hal_internal_vsync_set_tear_mode  CVWL668T.lib(hal_internal_vsync.o)
    0x00017008   0x00017008   0x0000006c   Code   RO          738    i.hal_internal_vsync_set_tx_state  CVWL668T.lib(hal_internal_vsync.o)
    0x00017074   0x00017074   0x0000006c   Code   RO          785    i.hal_intl_dcs_init_sw_fltr  CVWL668T.lib(hal_internal_dcs.o)
    0x000170e0   0x000170e0   0x0000044c   Code   RO          787    i.hal_intl_dcs_rx_get_dcs_packet_data  CVWL668T.lib(hal_internal_dcs.o)
    0x0001752c   0x0001752c   0x00000088   Code   RO          788    i.hal_intl_dcs_rx_receive_packet  CVWL668T.lib(hal_internal_dcs.o)
    0x000175b4   0x000175b4   0x00000174   Code   RO          789    i.hal_intl_dcs_rx_receive_pps  CVWL668T.lib(hal_internal_dcs.o)
    0x00017728   0x00017728   0x0000008c   Code   RO          790    i.hal_intl_dcs_set_auto_hw_filter  CVWL668T.lib(hal_internal_dcs.o)
    0x000177b4   0x000177b4   0x0000002c   Code   RO          792    i.hal_intl_dcs_sw_filter_handle  CVWL668T.lib(hal_internal_dcs.o)
    0x000177e0   0x000177e0   0x000002f0   Code   RO          813    i.hal_intl_fb_cal_fb_info  CVWL668T.lib(hal_internal_fb.o)
    0x00017ad0   0x00017ad0   0x00000064   Code   RO          814    i.hal_intl_fb_check_bandwidth  CVWL668T.lib(hal_internal_fb.o)
    0x00017b34   0x00017b34   0x000000dc   Code   RO          815    i.hal_intl_fb_edge_resize  CVWL668T.lib(hal_internal_fb.o)
    0x00017c10   0x00017c10   0x00000064   Code   RO          816    i.hal_intl_fb_flow_control_adapter  CVWL668T.lib(hal_internal_fb.o)
    0x00017c74   0x00017c74   0x0000000c   Code   RO          817    i.hal_intl_fb_get_memc_flow_mode  CVWL668T.lib(hal_internal_fb.o)
    0x00017c80   0x00017c80   0x00000010   Code   RO          818    i.hal_intl_fb_get_rx_fb_info  CVWL668T.lib(hal_internal_fb.o)
    0x00017c90   0x00017c90   0x00000010   Code   RO          819    i.hal_intl_fb_get_tx_fb_info  CVWL668T.lib(hal_internal_fb.o)
    0x00017ca0   0x00017ca0   0x0000000c   Code   RO          820    i.hal_intl_fb_get_user_flow  CVWL668T.lib(hal_internal_fb.o)
    0x00017cac   0x00017cac   0x00000028   Code   RO          838    i.hal_intl_svs_deinit_rx  CVWL668T.lib(hal_internal_svs.o)
    0x00017cd4   0x00017cd4   0x00000010   Code   RO          839    i.hal_intl_svs_deinit_tx  CVWL668T.lib(hal_internal_svs.o)
    0x00017ce4   0x00017ce4   0x00000024   Code   RO          840    i.hal_intl_svs_handle  CVWL668T.lib(hal_internal_svs.o)
    0x00017d08   0x00017d08   0x00000080   Code   RO          841    i.hal_intl_svs_init_rx  CVWL668T.lib(hal_internal_svs.o)
    0x00017d88   0x00017d88   0x00000014   Code   RO          842    i.hal_intl_svs_init_tx  CVWL668T.lib(hal_internal_svs.o)
    0x00017d9c   0x00017d9c   0x0000000c   Code   RO          844    i.hal_intl_svs_set_rx_vtt  CVWL668T.lib(hal_internal_svs.o)
    0x00017da8   0x00017da8   0x00000048   Code   RO          846    i.hal_intl_svs_update_rxbr_clk  CVWL668T.lib(hal_internal_svs.o)
    0x00017df0   0x00017df0   0x00000070   Code   RO          450    i.hal_lcdc_displayproc_config  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00017e60   0x00017e60   0x0000003e   Code   RO          451    i.hal_lcdc_init_cfg  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00017e9e   0x00017e9e   0x00000070   Code   RO          452    i.hal_lcdc_init_clk  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00017f0e   0x00017f0e   0x00000002   PAD
    0x00017f10   0x00017f10   0x00000128   Code   RO          453    i.hal_lcdc_postproc_config  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00018038   0x00018038   0x00000024   Code   RO          454    i.hal_lcdc_start    CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001805c   0x0001805c   0x0000003c   Code   RO          455    i.hal_lcdc_timinggen_config  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00018098   0x00018098   0x000000e0   Code   RO          456    i.hal_lcdc_upscaler_config  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00018178   0x00018178   0x000000bc   Code   RO          458    i.hal_nonshadow_func_update  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00018234   0x00018234   0x0000002a   Code   RO          623    i.hal_pwr_enter_deep_sleep_mode  CVWL668T.lib(hal_pwr.o)
    0x0001825e   0x0001825e   0x00000008   Code   RO          624    i.hal_pwr_enter_normal_sleep_mode  CVWL668T.lib(hal_pwr.o)
    0x00018266   0x00018266   0x00000002   PAD
    0x00018268   0x00018268   0x00000064   Code   RO          625    i.hal_pwr_enter_stop_sleep_mode  CVWL668T.lib(hal_pwr.o)
    0x000182cc   0x000182cc   0x0000000a   Code   RO          626    i.hal_pwr_exit_sleep_mode  CVWL668T.lib(hal_pwr.o)
    0x000182d6   0x000182d6   0x00000008   Code   RO          628    i.hal_pwr_get_vcc_power_ready  CVWL668T.lib(hal_pwr.o)
    0x000182de   0x000182de   0x00000008   Code   RO          633    i.hal_pwr_set_main_power  CVWL668T.lib(hal_pwr.o)
    0x000182e6   0x000182e6   0x00000008   Code   RO          635    i.hal_pwr_set_sleep_mode_power  CVWL668T.lib(hal_pwr.o)
    0x000182ee   0x000182ee   0x00000002   PAD
    0x000182f0   0x000182f0   0x00000064   Code   RO          636    i.hal_pwr_set_stop_sleep_wakeup_pin  CVWL668T.lib(hal_pwr.o)
    0x00018354   0x00018354   0x00000040   Code   RO          559    i.hal_swire_deinit  CVWL668T.lib(hal_swire.o)
    0x00018394   0x00018394   0x0000005c   Code   RO          560    i.hal_swire_enable  CVWL668T.lib(hal_swire.o)
    0x000183f0   0x000183f0   0x00000058   Code   RO          561    i.hal_swire_init    CVWL668T.lib(hal_swire.o)
    0x00018448   0x00018448   0x00000024   Code   RO          563    i.hal_swire_set_pulse  CVWL668T.lib(hal_swire.o)
    0x0001846c   0x0001846c   0x00000040   Code   RO          564    i.hal_swire_set_timer  CVWL668T.lib(hal_swire.o)
    0x000184ac   0x000184ac   0x000000e4   Code   RO          584    i.hal_system_init   CVWL668T.lib(hal_system.o)
    0x00018590   0x00018590   0x00000050   Code   RO          587    i.hal_system_updata_sysclk  CVWL668T.lib(hal_system.o)
    0x000185e0   0x000185e0   0x00000030   Code   RO          602    i.hal_timer_deinit  CVWL668T.lib(hal_timer.o)
    0x00018610   0x00018610   0x0000001c   Code   RO          604    i.hal_timer_init    CVWL668T.lib(hal_timer.o)
    0x0001862c   0x0001862c   0x00000008   Code   RO          605    i.hal_timer_set_repeat  CVWL668T.lib(hal_timer.o)
    0x00018634   0x00018634   0x00000030   Code   RO          459    i.hal_tx_frame_rate_adjust  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00018664   0x00018664   0x00000094   Code   RO          696    i.hal_uart_init     CVWL668T.lib(hal_uart.o)
    0x000186f8   0x000186f8   0x0000001c   Code   RO          699    i.hal_uart_send_blocking  CVWL668T.lib(hal_uart.o)
    0x00018714   0x00018714   0x00000018   Code   RO          460    i.hal_vsync_func_update  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001872c   0x0001872c   0x000000cc   Code   RO          740    i.hal_vsync_reset_lcdc_scaler  CVWL668T.lib(hal_internal_vsync.o)
    0x000187f8   0x000187f8   0x00000040   Code   RO            3    i.main              main.o
    0x00018838   0x00018838   0x0000007c   Code   RO          117    i.pps_update_handle  p6a_demo.o
    0x000188b4   0x000188b4   0x000002b8   Code   RO          741    i.rxbr_irq1_callback  CVWL668T.lib(hal_internal_vsync.o)
    0x00018b6c   0x00018b6c   0x0000003a   Code   RO          118    i.send_panel_init_code  p6a_demo.o
    0x00018ba6   0x00018ba6   0x00000002   PAD
    0x00018ba8   0x00018ba8   0x00000044   Code   RO          742    i.soft_double_buffer_update  CVWL668T.lib(hal_internal_vsync.o)
    0x00018bec   0x00018bec   0x0000007c   Code   RO          743    i.soft_gen_te       CVWL668T.lib(hal_internal_vsync.o)
    0x00018c68   0x00018c68   0x00000094   Code   RO          744    i.soft_gen_te_double_buffer  CVWL668T.lib(hal_internal_vsync.o)
    0x00018cfc   0x00018cfc   0x00000018   Code   RO          638    i.stop_sleep_cb     CVWL668T.lib(hal_pwr.o)
    0x00018d14   0x00018d14   0x000000ac   Code   RO          847    i.svs_direct_mode_setting  CVWL668T.lib(hal_internal_svs.o)
    0x00018dc0   0x00018dc0   0x0000001c   Code   RO          848    i.svs_get_rel_intv  CVWL668T.lib(hal_internal_svs.o)
    0x00018ddc   0x00018ddc   0x000000b0   Code   RO          849    i.svs_sync_handle   CVWL668T.lib(hal_internal_svs.o)
    0x00018e8c   0x00018e8c   0x000000cc   Code   RO          850    i.svs_wait_fr_stab  CVWL668T.lib(hal_internal_svs.o)
    0x00018f58   0x00018f58   0x0000010c   Code   RO          851    i.svs_wait_start    CVWL668T.lib(hal_internal_svs.o)
    0x00019064   0x00019064   0x00000034   Code   RO          673    i.tau_log_init      CVWL668T.lib(tau_log.o)
    0x00019098   0x00019098   0x00000084   Code   RO          674    i.tau_log_printf    CVWL668T.lib(tau_log.o)
    0x0001911c   0x0001911c   0x00000076   Code   RO          675    i.tau_log_push_log  CVWL668T.lib(tau_log.o)
    0x00019192   0x00019192   0x00000002   PAD
    0x00019194   0x00019194   0x000000b4   Code   RO          745    i.vidc_callback     CVWL668T.lib(hal_internal_vsync.o)
    0x00019248   0x00019248   0x00000118   Code   RO          746    i.vpre_err_reset    CVWL668T.lib(hal_internal_vsync.o)
    0x00019360   0x00019360   0x000020ac   Data   RO          121    .constdata          p6a_demo.o
    0x0001b40c   0x0001b40c   0x00000028   Data   RO          367    .constdata          CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x0001b434   0x0001b434   0x0000001c   Data   RO          463    .constdata          CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001b450   0x0001b450   0x0000004e   Data   RO          536    .constdata          CVWL668T.lib(hal_gpio.o)
    0x0001b49e   0x0001b49e   0x00000002   PAD
    0x0001b4a0   0x0001b4a0   0x00000030   Data   RO          701    .constdata          CVWL668T.lib(hal_uart.o)
    0x0001b4d0   0x0001b4d0   0x00000010   Data   RO         1798    .constdata          CVWL668T.lib(drv_uart.o)
    0x0001b4e0   0x0001b4e0   0x00000042   Data   RO          368    .conststring        CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x0001b522   0x0001b522   0x00000002   PAD
    0x0001b524   0x0001b524   0x00000090   Data   RO          748    .conststring        CVWL668T.lib(hal_internal_vsync.o)
    0x0001b5b4   0x0001b5b4   0x0000008e   Data   RO          795    .conststring        CVWL668T.lib(hal_internal_dcs.o)
    0x0001b642   0x0001b642   0x00000002   PAD
    0x0001b644   0x0001b644   0x00000020   Data   RO         2208    Region$$Table       anon$$obj.o


    Execution Region RW_IRAM1 (Exec base: 0x00070000, Load base: 0x0001b664, Size: 0x00003168, Max: 0x00008000, ABSOLUTE, COMPRESSED[0x0000016c])

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00070000   COMPRESSED   0x0000011f   Data   RW          122    .data               p6a_demo.o
    0x0007011f   COMPRESSED   0x00000001   PAD
    0x00070120   COMPRESSED   0x00000024   Data   RW          369    .data               CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00070144   COMPRESSED   0x0000005c   Data   RW          464    .data               CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x000701a0   COMPRESSED   0x00000002   Data   RW          566    .data               CVWL668T.lib(hal_swire.o)
    0x000701a2   COMPRESSED   0x00000002   PAD
    0x000701a4   COMPRESSED   0x00000008   Data   RW          639    .data               CVWL668T.lib(hal_pwr.o)
    0x000701ac   COMPRESSED   0x00000001   Data   RW          678    .data               CVWL668T.lib(tau_log.o)
    0x000701ad   COMPRESSED   0x00000003   PAD
    0x000701b0   COMPRESSED   0x00000018   Data   RW          702    .data               CVWL668T.lib(hal_uart.o)
    0x000701c8   COMPRESSED   0x00000010   Data   RW          749    .data               CVWL668T.lib(hal_internal_vsync.o)
    0x000701d8   COMPRESSED   0x00000028   Data   RW          796    .data               CVWL668T.lib(hal_internal_dcs.o)
    0x00070200   COMPRESSED   0x0000000c   Data   RW          880    .data               CVWL668T.lib(drv_common.o)
    0x0007020c   COMPRESSED   0x00000001   Data   RW          881    .data               CVWL668T.lib(drv_common.o)
    0x0007020d   COMPRESSED   0x00000003   PAD
    0x00070210   COMPRESSED   0x00000004   Data   RW          967    .data               CVWL668T.lib(drv_gpio.o)
    0x00070214   COMPRESSED   0x00000004   Data   RW         1119    .data               CVWL668T.lib(drv_swire.o)
    0x00070218   COMPRESSED   0x00000050   Data   RW         1167    .data               CVWL668T.lib(drv_timer.o)
    0x00070268   COMPRESSED   0x00000004   Data   RW         1208    .data               CVWL668T.lib(drv_se.o)
    0x0007026c   COMPRESSED   0x00000001   Data   RW         1248    .data               CVWL668T.lib(drv_dsi_rx.o)
    0x0007026d   COMPRESSED   0x00000003   PAD
    0x00070270   COMPRESSED   0x00000008   Data   RW         1583    .data               CVWL668T.lib(drv_rxbr.o)
    0x00070278   COMPRESSED   0x00000004   Data   RW         1670    .data               CVWL668T.lib(drv_vidc.o)
    0x0007027c   COMPRESSED   0x00000190   Data   RW         1745    .data               CVWL668T.lib(drv_dma.o)
    0x0007040c   COMPRESSED   0x00000004   Data   RW         2184    .data               mc_p.l(stdout.o)
    0x00070410        -       0x000000d0   Zero   RW          366    .bss                CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x000704e0        -       0x000000b8   Zero   RW          462    .bss                CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00070598        -       0x00000100   Zero   RW          677    .bss                CVWL668T.lib(tau_log.o)
    0x00070698        -       0x00000028   Zero   RW          747    .bss                CVWL668T.lib(hal_internal_vsync.o)
    0x000706c0        -       0x00000800   Zero   RW          793    .bss                CVWL668T.lib(hal_internal_dcs.o)
    0x00070ec0        -       0x000000ff   Zero   RW          794    .bss                CVWL668T.lib(hal_internal_dcs.o)
    0x00070fbf   COMPRESSED   0x00000001   PAD
    0x00070fc0        -       0x00000044   Zero   RW          822    .bss                CVWL668T.lib(hal_internal_fb.o)
    0x00071004        -       0x00000044   Zero   RW          852    .bss                CVWL668T.lib(hal_internal_svs.o)
    0x00071048        -       0x00000040   Zero   RW          966    .bss                CVWL668T.lib(drv_gpio.o)
    0x00071088        -       0x0000106c   Zero   RW         1191    .bss                CVWL668T.lib(dcs_packet_fifo.o)
    0x000720f4        -       0x00000010   Zero   RW         1743    .bss                CVWL668T.lib(drv_dma.o)
    0x00072104        -       0x00000060   Zero   RW         1797    .bss                CVWL668T.lib(drv_uart.o)
    0x00072164   COMPRESSED   0x00000004   PAD
    0x00072168        -       0x00001000   Zero   RW          321    STACK               startup_armcm0.o


==============================================================================

Image component sizes


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Object Name

        24          4          0          0          0        577   board.o
        64         32          0          0          0      10479   main.o
      2918        816       8364        287          0      31064   p6a_demo.o
       120         18        192          0       4096       2164   startup_armcm0.o

    ----------------------------------------------------------------------
      3132        870       8588        288       4096      44284   Object Totals
         0          0         32          0          0          0   (incl. Generated)
         6          0          0          1          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Member Name

       216         32          0          0       4204        252   dcs_packet_fifo.o
       104         62         28         13          0        192   drv_common.o
       536         90          0          0          0        792   drv_crgu.o
       136         22          0        400         16        196   drv_dma.o
       144         34          0          0          0        248   drv_dsc_dec.o
      1904        682          0          1          0       1340   drv_dsi_rx.o
      1704        306          0          0          0       2036   drv_dsi_tx.o
       148          0          0          0          0        260   drv_efuse.o
       340         50          0          4         64       1132   drv_gpio.o
      1080        166          0          0          0       1620   drv_lcdc.o
       658        104          0          0          0       1240   drv_memc.o
        40          0          0          0          0        120   drv_phy_common.o
       592        132          0          0          0        716   drv_pwr.o
       514        102          0          8          0       1120   drv_rxbr.o
      1012        264          0          4          0        492   drv_se.o
       264         54          0          4          0        560   drv_swire.o
       220         40          0          0          0        428   drv_sys_cfg.o
       366         38          0         80          0        816   drv_timer.o
      1172         54         16          0         96        980   drv_uart.o
       824        152          0          4          0       1700   drv_vidc.o
      2750        202        106         36        208       1256   hal_dsi_rx_ctrl.o
      4302        336         50         92        184       2212   hal_dsi_tx_ctrl.o
       548         40         78          0          0        828   hal_gpio.o
      2184        512        142         40       2303        656   hal_internal_dcs.o
      1292         60          0          0         68        688   hal_internal_fb.o
      1172        182          0          0         68        840   hal_internal_svs.o
      3400        716        144         16         40       1564   hal_internal_vsync.o
       308         32          0          8          0        616   hal_pwr.o
       344         32          0          2          0        348   hal_swire.o
       308         56          0          0          0        136   hal_system.o
        84          0          0          0          0        204   hal_timer.o
       176         18         48         24          0        144   hal_uart.o
        68          4          0          0          0        136   tau_delay.o
       354         30         16          1        256        320   tau_log.o
       200         20          0          0          0         76   ceil.o
        86          0          0          0          0          0   __dczerorl2.o
         0          0          0          0          0          0   entry.o
         0          0          0          0          0          0   entry10a.o
         0          0          0          0          0          0   entry11a.o
         8          4          0          0          0          0   entry2.o
         4          0          0          0          0          0   entry5.o
         0          0          0          0          0          0   entry7b.o
         0          0          0          0          0          0   entry8b.o
         8          4          0          0          0          0   entry9a.o
        30          0          0          0          0          0   handlers.o
        40          0          0          0          0         72   idiv.o
        36          8          0          0          0         68   init.o
         0          0          0          0          0          0   iusefp.o
        32          0          0          0          0         68   llshl.o
        38          0          0          0          0         68   llsshr.o
        34          0          0          0          0         68   llushr.o
        36          0          0          0          0         60   memcpya.o
        36          0          0          0          0        100   memseta.o
      2298        104          0          0          0        544   printfa.o
         0          0          0          4          0          0   stdout.o
        14          0          0          0          0         60   strlen.o
        44          0          0          0          0         72   uidiv.o
        96          0          0          0          0         84   uldiv.o
        40          2          0          0          0         68   cdrcmple.o
        20          0          0          0          0         68   cfcmple.o
        20          0          0          0          0         68   cfrcmple.o
        56          0          0          0          0         68   d2f.o
       356          4          0          0          0        140   dadd.o
       240          6          0          0          0         84   ddiv.o
       236          0          0          0          0        216   depilogue.o
        60         10          0          0          0         68   dfixui.o
        64         10          0          0          0         68   dfixul.o
        28          4          0          0          0         68   dfltui.o
       208          6          0          0          0         88   dmul.o
        40          0          0          0          0         60   f2d.o
       178          0          0          0          0        108   fadd.o
       124          0          0          0          0         72   fdiv.o
       130          0          0          0          0        144   fepilogue.o
        40          0          0          0          0         60   ffixui.o
        14          0          0          0          0         68   ffltui.o
       122          0          0          0          0         72   fmul.o
        24          0          0          0          0         60   fscalb.o

    ----------------------------------------------------------------------
     34336       4786        636        752       7512      29176   Library Totals
        32          0          8         11          5          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Name

     29264       4604        628        737       7507      26188   CVWL668T.lib
       200         20          0          0          0         76   m_ps.l
      2840        120          0          4          0       1264   mc_p.l
      2000         42          0          0          0       1648   mf_p.l

    ----------------------------------------------------------------------
     34336       4786        636        752       7512      29176   Library Totals

    ----------------------------------------------------------------------

==============================================================================


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   

     37468       5656       9224       1040      11608      53948   Grand Totals
     37468       5656       9224        364      11608      53948   ELF Image Totals (compressed)
     37468       5656       9224        364          0          0   ROM Totals

==============================================================================

    Total RO  Size (Code + RO Data)                46692 (  45.60kB)
    Total RW  Size (RW Data + ZI Data)             12648 (  12.35kB)
    Total ROM Size (Code + RO Data + RW Data)      47056 (  45.95kB)

==============================================================================

