Component: ARM Compiler 5.06 update 6 (build 750) Tool: armlink [4d35ed]

==============================================================================

Section Cross References

    main.o(i.main) refers to board.o(i.board_Init) for board_Init
    main.o(i.main) refers to p6a_demo.o(i.google_p6a_demo) for google_p6a_demo
    main.o(i.main) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.Gpio_swire_output) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    p6a_demo.o(i.Gpio_swire_output) refers to tau_delay.o(i.delayMs) for delayMs
    p6a_demo.o(i.Gpio_swire_output) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    p6a_demo.o(i.Gpio_swire_output) refers to tau_delay.o(i.delayUs) for delayUs
    p6a_demo.o(i.Panel_CCM) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) for hal_dsi_tx_ctrl_set_ccm
    p6a_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) for hal_dsi_rx_ctrl_send_ack_cmd
    p6a_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) for hal_dsi_rx_ctrl_get_max_ret_size
    p6a_demo.o(i.ap_dcs_read) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.ap_dcs_read) refers to p6a_demo.o(.data) for g_rx_ctrl_handle
    p6a_demo.o(i.ap_dcs_set_backlight) refers to idiv.o(.text) for __aeabi_idivmod
    p6a_demo.o(i.ap_dcs_set_backlight) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    p6a_demo.o(i.ap_dcs_set_backlight) refers to p6a_demo.o(.data) for rd_51_val
    p6a_demo.o(i.ap_dcs_set_display_off) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.ap_dcs_set_display_off) refers to p6a_demo.o(.data) for panel_display_done
    p6a_demo.o(i.ap_dcs_set_display_on) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    p6a_demo.o(i.ap_dcs_set_display_on) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to tau_delay.o(i.delayMs) for delayMs
    p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to hal_timer.o(i.hal_timer_deinit) for hal_timer_deinit
    p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to hal_timer.o(i.hal_timer_stop) for hal_timer_stop
    p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode) for hal_dsi_tx_ctrl_set_tear_mode
    p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to p6a_demo.o(.data) for g_tx_ctrl_handle
    p6a_demo.o(i.ap_dcs_set_exit_idle_mode) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) for hal_dsi_rx_ctrl_set_hw_cmd_filter
    p6a_demo.o(i.ap_dcs_set_exit_idle_mode) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.ap_dcs_set_exit_idle_mode) refers to p6a_demo.o(.data) for sg_exit_idle_mode_flag
    p6a_demo.o(i.ap_dcs_set_exit_sleep_mode) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.ap_dcs_set_frame_change) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode) for hal_dsi_tx_ctrl_set_tear_mode
    p6a_demo.o(i.ap_dcs_set_frame_change) refers to p6a_demo.o(.data) for g_tx_ctrl_handle
    p6a_demo.o(i.ap_rstn_pull_down_cb) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.ap_rstn_pull_down_cb) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    p6a_demo.o(i.ap_rstn_pull_down_cb) refers to p6a_demo.o(.data) for sg_system_suspend
    p6a_demo.o(i.ap_rstn_pull_high_cb) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    p6a_demo.o(i.ap_rstn_pull_high_cb) refers to p6a_demo.o(.data) for sg_system_resume
    p6a_demo.o(i.ap_set_FPS_B1) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    p6a_demo.o(i.app_display_init) refers to p6a_demo.o(i.app_mipi_rx_init) for app_mipi_rx_init
    p6a_demo.o(i.app_display_init) refers to hal_pwr.o(i.hal_pwr_get_vcc_power_ready) for hal_pwr_get_vcc_power_ready
    p6a_demo.o(i.app_display_init) refers to p6a_demo.o(i.app_gpio_init) for app_gpio_init
    p6a_demo.o(i.app_display_init) refers to p6a_demo.o(i.app_mipi_tx_init) for app_mipi_tx_init
    p6a_demo.o(i.app_display_init) refers to p6a_demo.o(i.app_mipi_tx_start) for app_mipi_tx_start
    p6a_demo.o(i.app_gpio_init) refers to hal_gpio.o(i.hal_gpio_config_pad) for hal_gpio_config_pad
    p6a_demo.o(i.app_gpio_init) refers to p6a_demo.o(.constdata) for .constdata
    p6a_demo.o(i.app_init_panel) refers to p6a_demo.o(i.app_tx_panel_reset) for app_tx_panel_reset
    p6a_demo.o(i.app_init_panel) refers to p6a_demo.o(i.send_panel_init_code) for send_panel_init_code
    p6a_demo.o(i.app_init_panel) refers to p6a_demo.o(.constdata) for panel_init_code
    p6a_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) for hal_dsi_rx_ctrl_create_handle
    p6a_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) for hal_dsi_rx_ctrl_pre_init_pps
    p6a_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    p6a_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    p6a_demo.o(i.app_mipi_rx_init) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.app_mipi_rx_init) refers to p6a_demo.o(.data) for g_rx_ctrl_handle
    p6a_demo.o(i.app_mipi_rx_init) refers to p6a_demo.o(.constdata) for g_cus_rx_dcs_execute_table
    p6a_demo.o(i.app_mipi_rx_init) refers to p6a_demo.o(i.ap_dcs_read) for ap_dcs_read
    p6a_demo.o(i.app_mipi_rx_init) refers to p6a_demo.o(i.pps_update_handle) for pps_update_handle
    p6a_demo.o(i.app_mipi_tx_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) for hal_dsi_tx_ctrl_create_handle
    p6a_demo.o(i.app_mipi_tx_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    p6a_demo.o(i.app_mipi_tx_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) for hal_dsi_tx_ctrl_set_overwrite_rgb
    p6a_demo.o(i.app_mipi_tx_init) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.app_mipi_tx_init) refers to p6a_demo.o(.data) for g_tx_ctrl_handle
    p6a_demo.o(i.app_mipi_tx_start) refers to p6a_demo.o(i.app_init_panel) for app_init_panel
    p6a_demo.o(i.app_mipi_tx_start) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    p6a_demo.o(i.app_mipi_tx_start) refers to tau_delay.o(i.delayMs) for delayMs
    p6a_demo.o(i.app_mipi_tx_start) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    p6a_demo.o(i.app_mipi_tx_start) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    p6a_demo.o(i.app_mipi_tx_start) refers to p6a_demo.o(i.soft_swire_init) for soft_swire_init
    p6a_demo.o(i.app_mipi_tx_start) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.app_mipi_tx_start) refers to p6a_demo.o(.data) for g_tx_ctrl_handle
    p6a_demo.o(i.app_system_process) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.app_system_process) refers to p6a_demo.o(i.app_system_suspend) for app_system_suspend
    p6a_demo.o(i.app_system_process) refers to p6a_demo.o(i.app_system_resume) for app_system_resume
    p6a_demo.o(i.app_system_process) refers to p6a_demo.o(.data) for sg_system_suspend
    p6a_demo.o(i.app_system_resume) refers to hal_pwr.o(i.hal_pwr_exit_sleep_mode) for hal_pwr_exit_sleep_mode
    p6a_demo.o(i.app_system_resume) refers to p6a_demo.o(i.app_display_init) for app_display_init
    p6a_demo.o(i.app_system_resume) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.app_system_suspend) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) for hal_dsi_tx_ctrl_stop
    p6a_demo.o(i.app_system_suspend) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) for hal_dsi_tx_ctrl_deinit
    p6a_demo.o(i.app_system_suspend) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) for hal_dsi_rx_ctrl_stop
    p6a_demo.o(i.app_system_suspend) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) for hal_dsi_rx_ctrl_deinit
    p6a_demo.o(i.app_system_suspend) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    p6a_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_set_sleep_mode_power) for hal_pwr_set_sleep_mode_power
    p6a_demo.o(i.app_system_suspend) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    p6a_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_enter_normal_sleep_mode) for hal_pwr_enter_normal_sleep_mode
    p6a_demo.o(i.app_system_suspend) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) for hal_pwr_set_stop_sleep_wakeup_pin
    p6a_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) for hal_pwr_enter_stop_sleep_mode
    p6a_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode) for hal_pwr_enter_deep_sleep_mode
    p6a_demo.o(i.app_system_suspend) refers to p6a_demo.o(.data) for g_tx_ctrl_handle
    p6a_demo.o(i.app_system_suspend) refers to p6a_demo.o(i.ap_rstn_pull_high_cb) for ap_rstn_pull_high_cb
    p6a_demo.o(i.app_tx_panel_reset) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    p6a_demo.o(i.app_tx_panel_reset) refers to tau_delay.o(i.delayMs) for delayMs
    p6a_demo.o(i.google_p6a_demo) refers to hal_pwr.o(i.hal_pwr_set_main_power) for hal_pwr_set_main_power
    p6a_demo.o(i.google_p6a_demo) refers to p6a_demo.o(i.app_display_init) for app_display_init
    p6a_demo.o(i.google_p6a_demo) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.google_p6a_demo) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) for hal_dsi_rx_ctrl_dcs_async_handler
    p6a_demo.o(i.google_p6a_demo) refers to p6a_demo.o(.data) for g_rx_ctrl_handle
    p6a_demo.o(i.pps_update_handle) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode) for hal_dsi_tx_ctrl_set_tear_mode
    p6a_demo.o(i.pps_update_handle) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) for hal_dsi_rx_ctrl_toggle_resolution
    p6a_demo.o(i.pps_update_handle) refers to p6a_demo.o(.data) for g_rx_ctrl_handle
    p6a_demo.o(i.send_panel_init_code) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) for hal_dsi_tx_ctrl_write_array_cmd
    p6a_demo.o(i.send_panel_init_code) refers to tau_delay.o(i.delayUs) for delayUs
    p6a_demo.o(i.soft_swire_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    p6a_demo.o(i.soft_swire_init) refers to tau_delay.o(i.delayMs) for delayMs
    p6a_demo.o(i.soft_swire_init) refers to p6a_demo.o(i.soft_swire_start) for soft_swire_start
    p6a_demo.o(i.soft_swire_init) refers to hal_timer.o(i.hal_timer_init) for hal_timer_init
    p6a_demo.o(i.soft_swire_init) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    p6a_demo.o(i.soft_swire_init) refers to p6a_demo.o(.data) for s_swire_pwm_counter
    p6a_demo.o(i.soft_swire_init) refers to p6a_demo.o(i.soft_swire_timer_callback) for soft_swire_timer_callback
    p6a_demo.o(i.soft_swire_start) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    p6a_demo.o(i.soft_swire_start) refers to tau_delay.o(i.delayUs) for delayUs
    p6a_demo.o(i.soft_swire_timer_callback) refers to p6a_demo.o(i.soft_swire_start) for soft_swire_start
    p6a_demo.o(i.soft_swire_timer_callback) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    p6a_demo.o(i.soft_swire_timer_callback) refers to hal_timer.o(i.hal_timer_deinit) for hal_timer_deinit
    p6a_demo.o(i.soft_swire_timer_callback) refers to hal_timer.o(i.hal_timer_stop) for hal_timer_stop
    p6a_demo.o(i.soft_swire_timer_callback) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    p6a_demo.o(i.soft_swire_timer_callback) refers to p6a_demo.o(.data) for s_swire_pwm_counter
    p6a_demo.o(i.soft_te_timer_cb) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) for hal_dsi_tx_ctrl_gen_a_tear_signal
    p6a_demo.o(i.soft_te_timer_cb) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    p6a_demo.o(i.soft_te_timer_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode) for hal_dsi_tx_ctrl_set_tear_mode
    p6a_demo.o(i.soft_te_timer_init) refers to hal_timer.o(i.hal_timer_init) for hal_timer_init
    p6a_demo.o(i.soft_te_timer_init) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    p6a_demo.o(i.soft_te_timer_init) refers to p6a_demo.o(.data) for g_tx_ctrl_handle
    p6a_demo.o(i.soft_te_timer_init) refers to p6a_demo.o(i.soft_te_timer_cb) for soft_te_timer_cb
    p6a_demo.o(.constdata) refers to p6a_demo.o(i.ap_dcs_set_display_on) for ap_dcs_set_display_on
    p6a_demo.o(.constdata) refers to p6a_demo.o(i.ap_dcs_set_display_off) for ap_dcs_set_display_off
    p6a_demo.o(.constdata) refers to p6a_demo.o(i.ap_dcs_set_backlight) for ap_dcs_set_backlight
    p6a_demo.o(.constdata) refers to p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) for ap_dcs_set_enter_sleep_mode
    p6a_demo.o(.constdata) refers to p6a_demo.o(i.ap_dcs_set_exit_sleep_mode) for ap_dcs_set_exit_sleep_mode
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_init) for hal_system_init
    board.o(i.board_Init) refers to tau_log.o(i.tau_log_init) for tau_log_init
    startup_armcm0.o(RESET) refers to startup_armcm0.o(STACK) for __initial_sp
    startup_armcm0.o(RESET) refers to startup_armcm0.o(.text) for Reset_Handler
    startup_armcm0.o(RESET) refers to drv_common.o(i.HardFault_Handler) for HardFault_Handler
    startup_armcm0.o(RESET) refers to drv_common.o(i.SysTick_Handler) for SysTick_Handler
    startup_armcm0.o(RESET) refers to drv_vidc.o(i.VIDC_IRQn_Handler) for VIDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to hal_internal_vsync.o(i.LCDC_IRQn_Handler) for LCDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) for MIPI_RX_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler) for MIPI_TX_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_memc.o(i.MEMC_IRQn_Handler) for MEMC_IRQn_Handler
    startup_armcm0.o(RESET) refers to hal_internal_dcs.o(i.VPRE_IRQn_Handler) for VPRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_dma.o(i.DMA_IRQn_Handler) for DMA_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER0_IRQn_Handler) for TIMER0_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER1_IRQn_Handler) for TIMER1_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER2_IRQn_Handler) for TIMER2_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER3_IRQn_Handler) for TIMER3_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_uart.o(i.UART_IRQn_Handler) for UART_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_rxbr.o(i.VPRE1_IRQn_Handler) for VPRE1_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.AP_NRESET_IRQn_Handler) for AP_NRESET_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT0_IRQn_Handler) for EXTI_INT0_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT1_IRQn_Handler) for EXTI_INT1_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT2_IRQn_Handler) for EXTI_INT2_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT3_IRQn_Handler) for EXTI_INT3_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT4_IRQn_Handler) for EXTI_INT4_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT5_IRQn_Handler) for EXTI_INT5_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT6_IRQn_Handler) for EXTI_INT6_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT7_IRQn_Handler) for EXTI_INT7_IRQn_Handler
    startup_armcm0.o(.text) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd) refers to drv_rxbr.o(i.drv_rxbr_set_ack_pkt_md) for drv_rxbr_set_ack_pkt_md
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_lpdt_fifo_status) for drv_dsi_rx_get_lpdt_fifo_status
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) for dcs_packet_get_fifo_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) for dcs_packet_free_fifo_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) for hal_internal_vsync_get_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_reset_modules) for drv_crgu_reset_modules
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_line) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_line) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_line) refers to hal_dsi_rx_ctrl.o(i.swap_uint16_t) for swap_uint16_t
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_line) refers to fflti.o(.text) for __aeabi_i2f
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_line) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_line) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data_ex) for hal_dsi_rx_ctrl_set_pixel_data_ex
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_rxbr.o(i.drv_rxbr_swpxl_clr) for drv_rxbr_swpxl_clr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_rxbr.o(i.drv_rxbr_set_cmd_filter) for drv_rxbr_set_cmd_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_vidc.o(i.drv_vidc_set_src_parameter) for drv_vidc_set_src_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_vidc.o(i.drv_vidc_set_pu_ctrl) for drv_vidc_set_pu_ctrl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_rxbr.o(i.drv_rxbr_set_swpxl_data) for drv_rxbr_set_swpxl_data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg) for drv_dsi_rx_set_ddi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) for hal_dsi_rx_ctrl_set_rx_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg) for drv_dsi_rx_set_ipi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.constdata) for .constdata
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_force_video_crtl) refers to drv_dsi_rx.o(i.drv_dsi_rx_force_video_crtl) for drv_dsi_rx_force_video_crtl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_cap_pixel_color) refers to drv_vidc.o(i.drv_vidc_get_status2) for drv_vidc_get_status2
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size) for drv_dsi_rx_get_max_ret_size
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) for hal_dsi_rx_ctrl_init_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_rx) for hal_internal_vsync_init_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) for hal_dsi_rx_ctrl_init_dsi_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) for hal_dsi_rx_ctrl_init_rxbr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_irqen) for drv_dsc_dec_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) for hal_dsi_rx_ctrl_init_vidc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) for hal_dsi_rx_ctrl_init_memc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_se.o(i.drv_se_start_rx) for drv_se_start_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_pwr.o(i.drv_pwr_set_pll_clk) for drv_pwr_set_pll_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_clk) for drv_crgu_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dsc_clk) for drv_crgu_set_dsc_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_vidc_clk) for drv_crgu_set_vidc_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_fb_clk) for drv_crgu_set_fb_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg) for drv_dsi_rx_set_ctrl_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) for drv_dsi_rx_set_up_phy
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap) for drv_dsi_rx_set_lane_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_crc_en) for drv_dsi_rx_set_ddi_crc_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_ycbcr_frmt) for drv_dsi_rx_set_ipi_ycbcr_frmt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_tear_resp_en) for drv_dsi_rx_set_tear_resp_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_inten) for drv_dsi_rx_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc) for drv_dsi_rx_set_check_crc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt) for drv_dsi_rx_set_resp_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_mode) for drv_memc_set_ltpo_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_fs_en_conditions) for drv_memc_set_fs_en_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_lcdc_st_conditions) for drv_memc_set_lcdc_st_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_vidc_sync_cnt) for drv_memc_set_vidc_sync_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_double_buffer) for drv_memc_set_double_buffer
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_circ_mode_enable) for drv_memc_set_circ_mode_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_active_height) for drv_memc_set_active_height
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_pu_thres) for drv_memc_set_ltpo_pu_thres
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_color_format) for drv_rxbr_set_color_format
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th) for drv_rxbr_set_ltpo_drop_th
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_cfg) for drv_rxbr_set_usr_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_col) for drv_rxbr_set_usr_col
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_row) for drv_rxbr_set_usr_row
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg) for drv_rxbr_hline_rcv_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) for hal_intl_dcs_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_src_parameter) for drv_vidc_set_src_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pentile_swap) for drv_vidc_set_pentile_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_dst_parameter) for drv_vidc_set_dst_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_circ_mode_enable) for drv_vidc_set_circ_mode_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_init_module_enable) for drv_vidc_init_module_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_dither_config) for drv_vidc_set_dither_config
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_vintp_config) for drv_vidc_set_vintp_config
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_rotation) for drv_vidc_set_rotation
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef0) for drv_vidc_set_scld_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef1) for drv_vidc_set_scld_hcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef0) for drv_vidc_set_scld_vcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef1) for drv_vidc_set_scld_vcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_honly_hinitr) for drv_vidc_set_honly_hinitr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_honly_hinitb) for drv_vidc_set_honly_hinitb
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_honly_hcoef0) for drv_vidc_set_honly_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_mirror) for drv_vidc_set_mirror
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pu_ctrl) for drv_vidc_set_pu_ctrl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_dsi_rx_ctrl.o(.constdata) for .constdata
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to hal_internal_vsync.o(i.hal_internal_sync_register_rx_callback) for hal_internal_sync_register_rx_callback
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to drv_vidc.o(i.drv_vidc_set_irq_line) for drv_vidc_set_irq_line
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_write_cmd_entry) refers to hal_internal_dcs.o(i.hal_intl_dcs_register_write_cmd_entry) for hal_intl_dcs_register_write_cmd_entry
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header) for drv_rxbr_set_ack_pkt_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack) refers to drv_rxbr.o(i.drv_rxbr_set_cmd_response) for drv_rxbr_set_cmd_response
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) for hal_intl_dcs_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cap_pixel_pos) refers to drv_vidc.o(i.drv_vidc_debug_cap_pixel) for drv_vidc_debug_cap_pixel
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_check_crc) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc) for drv_dsi_rx_set_check_crc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_check_crc) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) for drv_dsi_rx_calc_ipi_tx_delay
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg) for drv_dsi_rx_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_log_level) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_drv_log_level) for drv_dsi_rx_set_drv_log_level
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to drv_rxbr.o(i.drv_rxbr_sw_reset) for drv_rxbr_sw_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data_ex) refers to drv_rxbr.o(i.drv_rxbr_sw_reset) for drv_rxbr_sw_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data_ex) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) for hal_dsi_rx_ctrl_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) for hal_intl_svs_update_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_clk) for drv_crgu_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_dsi_rx.o(i.drv_dsi_rx_power_up) for drv_dsi_rx_power_up
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) for hal_internal_vsync_toggle_input_frame_rate
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) for hal_internal_sync_input_resolution_change
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) for hal_dsi_tx_ctrl_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg) for drv_dsi_tx_phy_time_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) for drv_dsi_tx_phy_test_setup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready) for drv_dsi_tx_phy_status_ready
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_crgu.o(i.drv_crgu_reset_modules) for drv_crgu_reset_modules
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_reset_modules) for drv_crgu_reset_modules
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb) for hal_internal_sync_register_lcdc_cb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) for hal_internal_sync_set_fb_setting_manual
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) for hal_lcdc_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_frame) refers to drv_lcdc.o(i.drv_lcdc_fixed_frame_output) for drv_lcdc_fixed_frame_output
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_get_tear_mode) for drv_memc_get_tear_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_gen_a_tear_signal) for drv_memc_gen_a_tear_signal
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_tx) for hal_internal_vsync_init_tx
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb) for hal_internal_sync_register_lcdc_cb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) for hal_dsi_tx_ctrl_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) for hal_dsi_tx_init_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) for hal_dsi_tx_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) for hal_lcdc_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) for hal_lcdc_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready) for drv_dsi_tx_phy_status_ready
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) for hal_nonshadow_func_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_vsync_func_update) for hal_vsync_func_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_overwrite_enable) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_overwrite_enable) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_partial_disp_enable) refers to drv_lcdc.o(i.drv_lcdc_part_display_config) for drv_lcdc_part_display_config
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_partial_disp_enable) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload) for drv_dsi_tx_command_get_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) for hal_nonshadow_func_req_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_sync_line) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) for hal_internal_vsync_set_sync_line
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_sync_line) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) for hal_nonshadow_func_req_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) for hal_nonshadow_func_req_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) for hal_nonshadow_func_req_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb) for drv_lcdc_config_overwrite_rgb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_vpg) for drv_dsi_tx_set_vpg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) for hal_dsi_tx_ctrl_draw_flick
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp) for drv_dsi_tx_phy_clock_lane_auto_lp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_cfg_int_frame) for drv_lcdc_cfg_int_frame
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_enable_shadow_reg) for drv_lcdc_enable_shadow_reg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_start) for hal_lcdc_start
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_lcdc.o(i.drv_lcdc_stop_display) for drv_lcdc_stop_display
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) for hal_dsi_tx_ctrl_read_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg) for drv_dsi_tx_video_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack) for drv_dsi_tx_set_bta_ack
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time) for drv_dsi_tx_dpi_lpcmd_time
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode) for drv_dsi_tx_phy_lane_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode) for drv_dsi_tx_dpi_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity) for drv_dsi_tx_dpi_polarity
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_response_mode) for drv_dsi_tx_response_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div) for drv_dsi_tx_set_time_out_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg) for drv_dsi_tx_timeout_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp) for drv_dsi_tx_phy_clock_lane_auto_lp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_int) for drv_dsi_tx_config_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to drv_crgu.o(i.drv_crgu_set_dpi_clk) for drv_crgu_set_dpi_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to hal_dsi_tx_ctrl.o(.constdata) for .constdata
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg) for drv_dsi_tx_phy_time_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) for drv_dsi_tx_phy_test_setup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update) for hal_dsi_tx_timing_info_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) for hal_dsi_tx_cmd_mode_cal_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size) for drv_dsi_tx_edpi_cmd_size
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) for hal_dsi_tx_init_phy_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) for hal_dsi_tx_init_dpi_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) for hal_dsi_tx_vid_mode_cal_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing) for hal_dsi_tx_init_vid_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk) for drv_dsi_tx_set_video_chunk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing) for drv_dsi_tx_set_video_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_header) for drv_dsi_tx_command_header
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update) refers to d2f.o(.text) for __aeabi_d2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_internal_svs.o(i.hal_intl_svs_init_tx) for hal_intl_svs_init_tx
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) for hal_tx_frame_rate_adjust
    hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) refers to drv_lcdc.o(i.drv_lcdc_endianness_config) for drv_lcdc_endianness_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) refers to drv_lcdc.o(i.drv_lcdc_crop_hact) for drv_lcdc_crop_hact
    hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) for hal_lcdc_postproc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) for hal_lcdc_displayproc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) for hal_intl_fb_get_tx_fb_info
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) for hal_lcdc_timinggen_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to drv_lcdc.o(i.drv_lcdc_config_int) for drv_lcdc_config_int
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fscalb.o(.text) for __ARM_scalbnf
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_lcdc_clk) for drv_crgu_set_lcdc_clk
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) for hal_intl_fb_get_tx_fb_info
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) for hal_lcdc_upscaler_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_fldc_config) for drv_lcdc_fldc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_bcsa_config) for drv_lcdc_bcsa_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_fc_config) for drv_lcdc_fc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_edge_dect_config) for drv_lcdc_edge_dect_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_edge_enh_config) for drv_lcdc_edge_enh_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_vintp_mode_config) for drv_lcdc_vintp_mode_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_dith_config) for drv_lcdc_dith_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to drv_lcdc.o(i.drv_lcdc_vid_hw_start) for drv_lcdc_vid_hw_start
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to drv_lcdc.o(i.drv_lcdc_cmd_start) for drv_lcdc_cmd_start
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to drv_lcdc.o(i.drv_lcdc_ctrl_flow) for drv_lcdc_ctrl_flow
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to drv_lcdc.o(i.drv_lcdc_config_src_parameter) for drv_lcdc_config_src_parameter
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to drv_lcdc.o(i.drv_lcdc_set_prefetch) for drv_lcdc_set_prefetch
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for sg_pq_para
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_bcsa_config) for drv_lcdc_bcsa_config
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_fc_config) for drv_lcdc_fc_config
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_edge_dect_config) for drv_lcdc_edge_dect_config
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_edge_enh_config) for drv_lcdc_edge_enh_config
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for sg_pq_para
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to cfcmple.o(.text) for __aeabi_cfcmple
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_vsync_func_update) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_vsync_func_update) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_gpio.o(i.hal_gpio_config_pad) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_config_pad) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    hal_gpio.o(i.hal_gpio_config_pad) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    hal_gpio.o(i.hal_gpio_ctrl_eint) refers to drv_gpio.o(i.drv_gpio_set_int) for drv_gpio_set_int
    hal_gpio.o(i.hal_gpio_get_input_data) refers to drv_gpio.o(i.drv_gpio_get_input_data) for drv_gpio_get_input_data
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_eint) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group) for drv_sys_cfg_sel_gpio_group
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig) for drv_sys_cfg_sel_int_trig
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_init_input) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_input) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_init_output) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_reg_eint_cb) refers to drv_gpio.o(i.drv_gpio_register_callback) for drv_gpio_register_callback
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_gpio.o(i.drv_gpio_register_ap_reset_callback) for drv_gpio_register_ap_reset_callback
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) for drv_sys_cfg_sel_ap_rst_trig
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_high_impedance) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode) for drv_gpio_set_mode
    hal_gpio.o(i.hal_gpio_set_mode) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_output_data) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to hal_gpio.o(.constdata) for .constdata
    hal_system.o(i.hal_system_disable_systick) refers to drv_common.o(i.drv_common_disable_systick) for drv_common_disable_systick
    hal_system.o(i.hal_system_enable_systick) refers to drv_common.o(i.drv_common_enable_systick) for drv_common_enable_systick
    hal_system.o(i.hal_system_get_tick) refers to drv_common.o(i.drv_common_get_tick) for drv_common_get_tick
    hal_system.o(i.hal_system_idle_mode) refers to drv_common.o(i.drv_common_idle_mode) for drv_common_idle_mode
    hal_system.o(i.hal_system_init) refers to drv_pwr.o(i.drv_pwr_set_pll_clk) for drv_pwr_set_pll_clk
    hal_system.o(i.hal_system_init) refers to hal_system.o(i.hal_system_updata_sysclk) for hal_system_updata_sysclk
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_system.o(i.hal_system_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int) for drv_sys_cfg_clear_all_int
    hal_system.o(i.hal_system_init) refers to drv_common.o(i.drv_common_system_init) for drv_common_system_init
    hal_system.o(i.hal_system_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_system.o(i.hal_system_register_systick_cb) refers to drv_common.o(i.drv_common_systick_register_cb) for drv_common_systick_register_cb
    hal_system.o(i.hal_system_reset_chip) refers to drv_crgu.o(i.drv_crgu_reset_chip) for drv_crgu_reset_chip
    hal_system.o(i.hal_system_updata_sysclk) refers to drv_crgu.o(i.drv_crgu_set_ahb_clk) for drv_crgu_set_ahb_clk
    hal_system.o(i.hal_system_updata_sysclk) refers to drv_common.o(.data) for g_system_clock
    hal_system.o(i.hal_system_updata_sysclk) refers to drv_common.o(.data) for g_system_delay_step
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_set_repeat) for drv_timer_set_repeat
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_timer.o(i.hal_timer_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_timer.o(i.hal_timer_get_status) refers to drv_timer.o(i.drv_timer_get_status) for drv_timer_get_status
    hal_timer.o(i.hal_timer_init) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_timer.o(i.hal_timer_init) refers to drv_timer.o(i.drv_timer_set_prescaler) for drv_timer_set_prescaler
    hal_timer.o(i.hal_timer_set_repeat) refers to drv_timer.o(i.drv_timer_set_repeat) for drv_timer_set_repeat
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_pwr.o(i.hal_pwr_elvcc_close) refers to drv_pwr.o(i.drv_pwr_pwmled_electric_current) for drv_pwr_pwmled_electric_current
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_pwmled_electric_current) for drv_pwr_pwmled_electric_current
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_hv_ldo_mode_sel) for drv_pwr_hv_ldo_mode_sel
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_hv_ldo_mode_clock_sel) for drv_pwr_hv_ldo_mode_clock_sel
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_pwmled_driver_current_Big_step) for drv_pwr_pwmled_driver_current_Big_step
    hal_pwr.o(i.hal_pwr_elvcc_vol_set) refers to drv_pwr.o(i.drv_pwr_hv_ldo_voltage_set) for drv_pwr_hv_ldo_voltage_set
    hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode) refers to drv_pwr.o(i.drv_pwr_set_wakeup_type) for drv_pwr_set_wakeup_type
    hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode) for drv_pwr_enter_deep_sleep_mode
    hal_pwr.o(i.hal_pwr_enter_normal_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_sleep_mode_ex) for drv_pwr_enter_sleep_mode_ex
    hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_stop_sleep_mode) for drv_pwr_enter_stop_sleep_mode
    hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) refers to hal_pwr.o(.data) for .data
    hal_pwr.o(i.hal_pwr_exit_sleep_mode) refers to drv_pwr.o(i.drv_pwr_exit_sleep_mode) for drv_pwr_exit_sleep_mode
    hal_pwr.o(i.hal_pwr_get_reset_flag) refers to drv_crgu.o(i.drv_crgu_get_all_reset_flag) for drv_crgu_get_all_reset_flag
    hal_pwr.o(i.hal_pwr_get_reset_flag) refers to drv_pwr.o(i.drv_pwr_get_wakeflag) for drv_pwr_get_wakeflag
    hal_pwr.o(i.hal_pwr_get_reset_flag) refers to drv_crgu.o(i.drv_crgu_clear_all_reset_flags) for drv_crgu_clear_all_reset_flags
    hal_pwr.o(i.hal_pwr_get_vcc_power_ready) refers to drv_pwr.o(i.drv_pwr_get_power_ready_st) for drv_pwr_get_power_ready_st
    hal_pwr.o(i.hal_pwr_ldo13s_en) refers to drv_pwr.o(i.drv_pwr_ldo13s_en) for drv_pwr_ldo13s_en
    hal_pwr.o(i.hal_pwr_ldo13s_set) refers to drv_pwr.o(i.drv_pwr_ldo13s_set) for drv_pwr_ldo13s_set
    hal_pwr.o(i.hal_pwr_ldo18s_en) refers to drv_pwr.o(i.drv_pwr_ldo18s_en) for drv_pwr_ldo18s_en
    hal_pwr.o(i.hal_pwr_ldo18s_set) refers to drv_pwr.o(i.drv_pwr_ldo18s_set) for drv_pwr_ldo18s_set
    hal_pwr.o(i.hal_pwr_set_main_power) refers to drv_pwr.o(i.drv_pwr_set_digit_power_sel) for drv_pwr_set_digit_power_sel
    hal_pwr.o(i.hal_pwr_set_pvd) refers to drv_pwr.o(i.drv_pwr_set_pvd) for drv_pwr_set_pvd
    hal_pwr.o(i.hal_pwr_set_sleep_mode_power) refers to drv_pwr.o(i.drv_pwr_set_breath_screen_power_sel) for drv_pwr_set_breath_screen_power_sel
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_ctrl_eint) for hal_gpio_ctrl_eint
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_init_eint) for hal_gpio_init_eint
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_reg_eint_cb) for hal_gpio_reg_eint_cb
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_pwr.o(.data) for .data
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_pwr.o(i.stop_sleep_cb) for stop_sleep_cb
    hal_pwr.o(i.hal_pwr_set_vcc_enable) refers to drv_pwr.o(i.drv_pwr_charge_pump_en) for drv_pwr_charge_pump_en
    hal_pwr.o(i.stop_sleep_cb) refers to hal_pwr.o(.data) for .data
    tau_delay.o(i.delayMs) refers to tau_delay.o(i.delayUs) for delayUs
    tau_delay.o(i.delayUs) refers to drv_common.o(.data) for g_system_delay_step
    tau_log.o(i.fgetc) refers to hal_uart.o(i.hal_uart_recv_blocking) for hal_uart_recv_blocking
    tau_log.o(i.fgetc) refers to hal_system.o(i.hal_system_get_debug_state) for hal_system_get_debug_state
    tau_log.o(i.fgetc) refers to hal_system.o(i.hal_system_clear_debug_state) for hal_system_clear_debug_state
    tau_log.o(i.fgetc) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.fputc) refers to tau_log.o(i.tau_log_push_log) for tau_log_push_log
    tau_log.o(i.fputc) refers to hal_uart.o(i.hal_uart_send_blocking) for hal_uart_send_blocking
    tau_log.o(i.fputc) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.tau_log_init) refers to hal_uart.o(i.hal_uart_init) for hal_uart_init
    tau_log.o(i.tau_log_init) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.tau_log_printf) refers to memseta.o(.text) for __aeabi_memclr4
    tau_log.o(i.tau_log_printf) refers to strlen.o(.text) for strlen
    tau_log.o(i.tau_log_printf) refers to printfa.o(i.__0vsprintf) for vsprintf
    tau_log.o(i.tau_log_printf) refers to tau_log.o(i.tau_log_push_log) for tau_log_push_log
    tau_log.o(i.tau_log_printf) refers to printfa.o(i.__0printf) for __2printf
    tau_log.o(i.tau_log_printf) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.tau_log_printf) refers to tau_log.o(.bss) for g_log_buf
    tau_log.o(i.tau_log_push_log) refers to memcpya.o(.text) for __aeabi_memcpy
    tau_log.o(i.tau_log_push_log) refers to tau_delay.o(i.delayUs) for delayUs
    tau_log.o(.ARM.__at_0x1101C) refers to tau_log.o(.bss) for g_log_buf
    hal_uart.o(i.hal_uart0_rx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart0_tx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart1_rx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart1_tx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_deinit) refers to drv_uart.o(i.drv_uart_deinit) for drv_uart_deinit
    hal_uart.o(i.hal_uart_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_uart.o(i.hal_uart_deinit) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_dma_path_close) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_uart.o(i.hal_uart_dma_path_close) refers to drv_dma.o(i.drv_dma_deinit) for drv_dma_deinit
    hal_uart.o(i.hal_uart_dma_path_close) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_apply_handle) for drv_dma_apply_handle
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_set_burst) for drv_dma_set_burst
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_register_callback) for drv_dma_register_callback
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_enable_int) for drv_dma_enable_int
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_set_mem_trans_info) for drv_dma_set_mem_trans_info
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_enable) for drv_dma_enable
    hal_uart.o(i.hal_uart_dma_recv) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_uart.o(i.hal_uart_dma_recv) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_dma_recv) refers to hal_uart.o(i.hal_uart0_rx_dma_cb) for hal_uart0_rx_dma_cb
    hal_uart.o(i.hal_uart_dma_recv) refers to hal_uart.o(i.hal_uart1_rx_dma_cb) for hal_uart1_rx_dma_cb
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_apply_handle) for drv_dma_apply_handle
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_set_burst) for drv_dma_set_burst
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_register_callback) for drv_dma_register_callback
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_enable_int) for drv_dma_enable_int
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_set_mem_trans_info) for drv_dma_set_mem_trans_info
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_enable) for drv_dma_enable
    hal_uart.o(i.hal_uart_dma_send) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_uart.o(i.hal_uart_dma_send) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_dma_send) refers to hal_uart.o(i.hal_uart0_tx_dma_cb) for hal_uart0_tx_dma_cb
    hal_uart.o(i.hal_uart_dma_send) refers to hal_uart.o(i.hal_uart1_tx_dma_cb) for hal_uart1_tx_dma_cb
    hal_uart.o(i.hal_uart_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_uart.o(i.hal_uart_init) refers to drv_uart.o(i.drv_uart_init) for drv_uart_init
    hal_uart.o(i.hal_uart_init) refers to drv_uart.o(i.drv_uart_trans_create_handle) for drv_uart_trans_create_handle
    hal_uart.o(i.hal_uart_init) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_init) refers to drv_common.o(.data) for g_system_clock
    hal_uart.o(i.hal_uart_init) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_recv_blocking) refers to drv_uart.o(i.drv_uart_recv_blocking) for drv_uart_recv_blocking
    hal_uart.o(i.hal_uart_recv_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_recv_none_blocking) refers to drv_uart.o(i.drv_uart_recv_none_blocking) for drv_uart_recv_none_blocking
    hal_uart.o(i.hal_uart_recv_none_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_send_blocking) refers to drv_uart.o(i.drv_uart_send_blocking) for drv_uart_send_blocking
    hal_uart.o(i.hal_uart_send_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_send_none_blocking) refers to drv_uart.o(i.drv_uart_send_none_blocking) for drv_uart_send_none_blocking
    hal_uart.o(i.hal_uart_send_none_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_internal_vsync.o(i.LCDC_IRQn_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.LCDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_internal_vsync.o(i.LCDC_IRQn_Handler) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) for hal_intl_fb_cal_fb_info
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) for hal_dsi_tx_ctrl_gen_a_tear_signal
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_delay.o(i.delayUs) for delayUs
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) for hal_vsync_reset_lcdc_scaler
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_sync_register_rx_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) for hal_intl_fb_set_fb_info_manual
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) for hal_intl_fb_cal_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_svs.o(i.hal_intl_svs_init_rx) for hal_intl_svs_init_rx
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr) for hal_intl_dcs_init_sw_fltr
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_rxbr.o(i.drv_rxbr_register_irq1_callback) for drv_rxbr_register_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_vidc.o(i.drv_vidc_register_callback) for drv_vidc_register_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_init) for dcs_packet_fifo_init
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_pro_motion_init) for soft_pro_motion_init
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_gen_te) for soft_gen_te
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.rxbr_irq1_callback) for rxbr_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.vidc_callback) for vidc_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_gen_te_double_buffer) for soft_gen_te_double_buffer
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) for hal_intl_fb_cal_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_svs.o(i.hal_intl_svs_deinit_rx) for hal_intl_svs_deinit_rx
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_svs.o(i.hal_intl_svs_set_sync_coef) for hal_intl_svs_set_sync_coef
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_memc.o(i.drv_memc_set_frame_drop_select) for drv_memc_set_frame_drop_select
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_set_tear_line) for drv_lcdc_set_tear_line
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to idiv.o(.text) for __aeabi_idivmod
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_config_acc_command_mode) for drv_lcdc_config_acc_command_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_svs.o(i.hal_intl_svs_deinit_tx) for hal_intl_svs_deinit_tx
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.soft_pro_motion_init) for soft_pro_motion_init
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_svs.o(i.hal_intl_svs_set_input_frate) for hal_intl_svs_set_input_frate
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg) for drv_rxbr_hline_rcv0_cfg
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dadd.o(.text) for __aeabi_dadd
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_internal_vsync.o(i.soft_pro_motion_init) for soft_pro_motion_init
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_int_source) for drv_rxbr_get_int_source
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.soft_double_buffer_update) for soft_double_buffer_update
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_svs.o(i.hal_intl_svs_handle) for hal_intl_svs_handle
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.vpre_err_reset) for vpre_err_reset
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_lcdc.o(i.drv_lcdc_cmd_start) for drv_lcdc_cmd_start
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt) for hal_intl_svs_set_rx_vtt
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.soft_double_buffer_update) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(i.soft_tear_adjust_line) for soft_tear_adjust_line
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.soft_gen_te_double_buffer) refers to hal_internal_vsync.o(i.soft_tear_adjust_line) for soft_tear_adjust_line
    hal_internal_vsync.o(i.soft_gen_te_double_buffer) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_pro_motion_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.soft_pro_motion_init) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_pro_motion_init) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.soft_tear_adjust_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_get_int_source) for drv_vidc_get_int_source
    hal_internal_vsync.o(i.vidc_callback) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_clear_irq) for drv_vidc_clear_irq
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_get_irq_status) for drv_vidc_get_irq_status
    hal_internal_vsync.o(i.vidc_callback) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.vpre_err_reset) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to hal_internal_dcs.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) for hal_intl_dcs_rx_receive_packet
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_dsc_dec.o(i.drv_dsc_dec_get_nslc) for drv_dsc_dec_get_nslc
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_crgu.o(i.drv_crgu_set_dsc_clk) for drv_crgu_set_dsc_clk
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to hal_internal_dcs.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr) refers to hal_internal_dcs.o(.bss) for .bss
    hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_register_write_cmd_entry) refers to hal_internal_dcs.o(.data) for .data
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle) for hal_intl_dcs_sw_filter_handle
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) for dcs_packet_fifo_alloc
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) for hal_dsi_rx_ctrl_dcs_async_handler
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_ddi_crc_en) for drv_dsi_rx_get_ddi_crc_en
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_dcs.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_dcs.o(.data) for .data
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) for hal_intl_dcs_rx_get_dcs_packet_data
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) for hal_intl_dcs_rx_receive_pps
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to hal_internal_dcs.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to memcmp.o(.text) for memcmp
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to hal_internal_dcs.o(.conststring) for .conststring
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) refers to memseta.o(.text) for __aeabi_memset
    hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) refers to drv_rxbr.o(i.drv_rxbr_set_filter_regs) for drv_rxbr_set_filter_regs
    hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) refers to hal_internal_dcs.o(.bss) for .bss
    hal_internal_dcs.o(i.hal_intl_dcs_set_dcs_direct_mode) refers to hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) for hal_intl_dcs_set_auto_hw_filter
    hal_internal_dcs.o(i.hal_intl_dcs_set_dcs_direct_mode) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle) refers to hal_internal_dcs.o(.data) for .data
    hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle) refers to hal_internal_dcs.o(.bss) for .bss
    hal_internal_dcs.o(.data) refers to hal_internal_dcs.o(.bss) for g_imm_buffer
    hal_internal_fb.o(i.ha_intl_fb_check_pu_size) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.ha_intl_fb_check_pu_size) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter) for hal_intl_fb_flow_control_adapter
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) for hal_intl_fb_check_bandwidth
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.ha_intl_fb_check_pu_size) for ha_intl_fb_check_pu_size
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.hal_intl_fb_edge_resize) for hal_intl_fb_edge_resize
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_fb.o(i.hal_intl_fb_edge_resize) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.hal_intl_fb_edge_resize) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_user_flow) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to hal_internal_fb.o(.conststring) for .conststring
    hal_internal_svs.o(i.hal_intl_svs_deinit_rx) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.hal_intl_svs_deinit_rx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_deinit_rx) refers to hal_internal_svs.o(i.svs_wait_start) for svs_wait_start
    hal_internal_svs.o(i.hal_intl_svs_deinit_tx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_handle) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) for hal_intl_svs_update_rxbr_clk
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_svs.o(i.svs_wait_start) for svs_wait_start
    hal_internal_svs.o(i.hal_intl_svs_init_tx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_svs.o(i.svs_wait_start) for svs_wait_start
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_svs.o(i.svs_wait_fr_stab) for svs_wait_fr_stab
    hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_set_sync_coef) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to dmul.o(.text) for __aeabi_dmul
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg) for drv_rxbr_hline_rcv1_cfg
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_get_rel_intv) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_svs.o(i.svs_get_rel_intv) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_sync_handle) refers to hal_internal_svs.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_svs.o(i.svs_sync_handle) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_svs.o(i.svs_sync_handle) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_svs.o(i.svs_sync_handle) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_svs.o(i.svs_sync_handle) refers to f2d.o(.text) for __aeabi_f2d
    hal_internal_svs.o(i.svs_sync_handle) refers to dadd.o(.text) for __aeabi_dadd
    hal_internal_svs.o(i.svs_sync_handle) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_svs.o(i.svs_sync_handle) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to hal_internal_svs.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to ffixui.o(.text) for __aeabi_f2uiz
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to hal_internal_svs.o(i.svs_sync_handle) for svs_sync_handle
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_svs.o(i.svs_wait_start) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_internal_svs.o(i.svs_wait_start) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_svs.o(i.svs_wait_start) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_internal_svs.o(i.svs_wait_start) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_svs.o(i.svs_wait_start) refers to f2d.o(.text) for __aeabi_f2d
    hal_internal_svs.o(i.svs_wait_start) refers to ceil.o(i.ceil) for ceil
    hal_internal_svs.o(i.svs_wait_start) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(i.svs_direct_mode_setting) for svs_direct_mode_setting
    hal_internal_svs.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_svs.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg) for drv_rxbr_hline_rcv1_cfg
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(i.svs_wait_fr_stab) for svs_wait_fr_stab
    drv_common.o(i.HardFault_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_common.o(i.SysTick_Handler) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_enable_systick) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_common.o(i.drv_common_enable_systick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_get_tick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_system_init) refers to drv_se.o(i.drv_se_init) for drv_se_init
    drv_common.o(i.drv_common_systick_register_cb) refers to drv_common.o(.data) for .data
    drv_crgu.o(i.drv_crgu_get_rxbr_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_crgu.o(i.drv_crgu_get_system_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to drv_se.o(i.drv_se_set_dsc) for drv_se_set_dsc
    drv_gpio.o(i.AP_NRESET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.AP_NRESET_IRQn_Handler) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.EXTI_INT0_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT1_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT2_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT3_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT4_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT5_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT6_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT7_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.drv_gpio_handle_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.drv_gpio_handle_int) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_register_ap_reset_callback) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.drv_gpio_register_callback) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_pwr.o(i.drv_pwr_analog_pwm_en) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_elvcc_pwm_en) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_elvcc_pwm_en) refers to tau_delay.o(i.delayMs) for delayMs
    drv_pwr.o(i.drv_pwr_enter_sleep_mode) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_enter_sleep_mode) refers to drv_pwr.o(i.drv_pwr_por_mode_flag) for drv_pwr_por_mode_flag
    drv_pwr.o(i.drv_pwr_enter_stop_sleep_mode) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_exit_sleep_mode) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_hv_ldo_mode_clock_sel) refers to drv_pwr.o(i.drv_pwr_hv_ldo_10M_clock) for drv_pwr_hv_ldo_10M_clock
    drv_pwr.o(i.drv_pwr_pwm_output_pwm_led) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_breath_screen_power_sel) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_digit_power_sel) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_system_clk) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_wakeup_type) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_sys_cfg.o(i.drv_sys_cfg_sel_dma_req) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_timer.o(i.TIMER0_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.TIMER1_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.TIMER2_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.TIMER3_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_timer.o(i.drv_timer_enable) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_get_instance) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_get_status) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_clear_status_flags) for drv_timer_clear_status_flags
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_register_callback) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_compare_val) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_compare_val) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_timer.o(i.drv_timer_set_compare_val) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_compare_val) refers to drv_common.o(.data) for g_system_clock
    drv_timer.o(i.drv_timer_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_repeat) refers to drv_timer.o(.data) for .data
    dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_fifo_init) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_size) refers to dcs_packet_fifo.o(.bss) for .bss
    drv_se.o(i.drv_se_init) refers to drv_efuse.o(i.drv_efuse_enter_inactive) for drv_efuse_enter_inactive
    drv_se.o(i.drv_se_init) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_se.o(i.drv_se_init) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_dsc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_dsc) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_lcdc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_lcdc) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_memc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_memc) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_rxbr) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_rxbr) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_vidc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_vidc) refers to drv_se.o(.data) for .data
    drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) refers to drv_dsi_rx.o(.data) for .data
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) for drv_dsi_rx_get_color_bpp
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to ffltui.o(.text) for __aeabi_ui2f
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fdiv.o(.text) for __aeabi_fdiv
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fmul.o(.text) for __aeabi_fmul
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc) for drv_dsi_rx_get_color_pcc
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fadd.o(.text) for __aeabi_fadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to cfrcmple.o(.text) for __aeabi_cfrcmple
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to f2d.o(.text) for __aeabi_f2d
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dadd.o(.text) for __aeabi_dadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dfixui.o(.text) for __aeabi_d2uiz
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_set_drv_log_level) refers to drv_dsi_rx.o(.data) for .data
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_test_lock) for drv_phy_test_lock
    drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_enter) for drv_tx_phy_test_enter
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_code) for drv_tx_phy_test_write_code
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_exit) for drv_tx_phy_test_exit
    drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_version) for drv_dsi_tx_version
    drv_dsi_tx.o(i.drv_dsi_tx_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_tx.o(i.drv_dsi_tx_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_lcdc.o(i.drv_lcdc_clear_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_lcdc.o(i.drv_lcdc_cmd_start) refers to drv_se.o(i.drv_se_set_lcdc) for drv_se_set_lcdc
    drv_lcdc.o(i.drv_lcdc_ctrl_flow) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    drv_lcdc.o(i.drv_lcdc_part_display_config) refers to drv_lcdc.o(i.drv_lcdc_pixel_value_config) for drv_lcdc_pixel_value_config
    drv_lcdc.o(i.drv_lcdc_set_int) refers to drv_lcdc.o(i.drv_lcdc_clear_int) for drv_lcdc_clear_int
    drv_lcdc.o(i.drv_lcdc_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_lcdc.o(i.drv_lcdc_vid_hw_start) refers to drv_se.o(i.drv_se_set_lcdc) for drv_se_set_lcdc
    drv_memc.o(i.MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_get_status) for drv_memc_get_status
    drv_memc.o(i.MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_clear_status) for drv_memc_clear_status
    drv_memc.o(i.MEMC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_memc.o(i.drv_memc_rate_transfer_sel) refers to drv_se.o(i.drv_se_set_memc) for drv_se_set_memc
    drv_memc.o(i.drv_memc_set_ltpo_mode) refers to drv_se.o(i.drv_se_set_memc) for drv_se_set_memc
    drv_rxbr.o(i.VPRE1_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.VPRE1_IRQn_Handler) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_EnableIRQ) for __NVIC_EnableIRQ
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_rxbr.o(i.drv_rxbr_register_irq0_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_register_irq1_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_set_cmd_filter) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_rxbr.o(i.drv_rxbr_set_cmd_response) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_rxbr.o(i.drv_rxbr_set_color_format) refers to drv_se.o(i.drv_se_set_rxbr) for drv_se_set_rxbr
    drv_rxbr.o(i.drv_rxbr_soft_reset) refers to tau_delay.o(i.delayMs) for delayMs
    drv_rxbr.o(i.drv_rxbr_sw_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_rxbr.o(i.drv_rxbr_sw_reset) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    drv_vidc.o(i.VIDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.VIDC_IRQn_Handler) refers to drv_vidc.o(.data) for .data
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_vidc.o(i.drv_vidc_register_callback) refers to drv_vidc.o(.data) for .data
    drv_vidc.o(i.drv_vidc_set_src_parameter) refers to drv_se.o(i.drv_se_set_vidc) for drv_se_set_vidc
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(i.drv_dma_get_int_source) for drv_dma_get_int_source
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(i.drv_dma_clear_status) for drv_dma_clear_status
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(.data) for .data
    drv_dma.o(i.drv_dma_apply_handle) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dma.o(i.drv_dma_apply_handle) refers to drv_dma.o(.data) for .data
    drv_dma.o(i.drv_dma_apply_handle) refers to drv_dma.o(.constdata) for .constdata
    drv_dma.o(i.drv_dma_deinit) refers to drv_dma.o(i.drv_dma_disable_int) for drv_dma_disable_int
    drv_dma.o(i.drv_dma_disable_int) refers to drv_dma.o(i.drv_dma_int_list_delete) for drv_dma_int_list_delete
    drv_dma.o(i.drv_dma_disable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.drv_dma_enable_int) refers to drv_dma.o(i.drv_dma_int_list_inset) for drv_dma_int_list_inset
    drv_dma.o(i.drv_dma_enable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dma.o(i.drv_dma_init) refers to drv_per_common.o(i.drv_per_set_clock) for drv_per_set_clock
    drv_dma.o(i.drv_dma_init) refers to drv_dma.o(i.drv_dma_update_handle_setting) for drv_dma_update_handle_setting
    drv_dma.o(i.drv_dma_int_list_delete) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_int_list_inset) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_update_handle_setting) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_dma_req) for drv_sys_cfg_sel_dma_req
    drv_dma.o(i.drv_dma_update_req_by_default) refers to drv_dma.o(i.drv_dma_update_handle_setting) for drv_dma_update_handle_setting
    drv_dma.o(i.drv_dma_update_req_by_default) refers to drv_dma.o(.constdata) for .constdata
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_int_trans_handle) for drv_uart_int_trans_handle
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_abort_recv) for drv_uart_abort_recv
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_abort_send) for drv_uart_abort_send
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(.constdata) for .constdata
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(i.drv_uart_reset_rx_fifo) for drv_uart_reset_rx_fifo
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(i.drv_uart_reset_tx_fifo) for drv_uart_reset_tx_fifo
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_deinit) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_deinit) refers to drv_uart.o(i.drv_uart_enable_clk) for drv_uart_enable_clk
    drv_uart.o(i.drv_uart_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.drv_uart_deinit) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_enable_clk) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    drv_uart.o(i.drv_uart_enable_int) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_enable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.drv_uart_get_def_cfg) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.drv_uart_get_def_cfg) refers to drv_common.o(.data) for g_system_clock
    drv_uart.o(i.drv_uart_get_instance) refers to drv_uart.o(.constdata) for .constdata
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_enable_clk) for drv_uart_enable_clk
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_set_baud_rate) for drv_uart_set_baud_rate
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_enable_int) for drv_uart_enable_int
    drv_uart.o(i.drv_uart_int_trans_handle) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_recv_none_blocking) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_recv_none_blocking) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_recv_none_blocking) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_reset_rx_fifo) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_reset_tx_fifo) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_send_none_blocking) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_send_none_blocking) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_send_none_blocking) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_set_baud_rate) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_uart.o(i.drv_uart_trans_create_handle) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_trans_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.drv_uart_trans_create_handle) refers to drv_uart.o(.bss) for .bss
    drv_efuse.o(i.drv_efuse_enter_inactive) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    drv_efuse.o(i.drv_efuse_enter_inactive) refers to drv_efuse.o(i.drv_efuse_int_enable) for drv_efuse_int_enable
    drv_efuse.o(i.drv_efuse_read) refers to drv_pwr.o(i.drv_pwr_efuse_pd) for drv_pwr_efuse_pd
    drv_efuse.o(i.drv_efuse_read) refers to drv_efuse.o(i.drv_efuse_read_req) for drv_efuse_read_req
    drv_efuse.o(i.drv_efuse_write) refers to drv_pwr.o(i.drv_pwr_efuse_pd) for drv_pwr_efuse_pd
    drv_efuse.o(i.drv_efuse_write) refers to drv_efuse.o(i.drv_efuse_write_req) for drv_efuse_write_req
    drv_efuse.o(i.drv_efuse_write_read_req_clear) refers to drv_efuse.o(i.drv_efuse_write_req) for drv_efuse_write_req
    drv_efuse.o(i.drv_efuse_write_read_req_clear) refers to drv_efuse.o(i.drv_efuse_read_req) for drv_efuse_read_req
    drv_per_common.o(i.drv_per_get_system_clk) refers to drv_crgu.o(i.drv_crgu_get_system_clk) for drv_crgu_get_system_clk
    drv_per_common.o(i.drv_per_reset_module) refers to drv_crgu.o(i.drv_crgu_reset_modules) for drv_crgu_reset_modules
    drv_per_common.o(i.drv_per_set_clock) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    ceil.o(i.__softfp_ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.__softfp_ceil) refers to ceil.o(i.ceil) for ceil
    ceil.o(i.ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.ceil) refers to dadd.o(.text) for __aeabi_dadd
    ceil.o(i.ceil) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry10a.o(.ARM.Collect$$$$0000000D) for __rt_final_cpp
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry11a.o(.ARM.Collect$$$$0000000F) for __rt_final_exit
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry7b.o(.ARM.Collect$$$$00000008) for _main_clock
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry8b.o(.ARM.Collect$$$$0000000A) for _main_cpp_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry9a.o(.ARM.Collect$$$$0000000B) for _main_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry5.o(.ARM.Collect$$$$00000004) for _main_scatterload
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry2.o(.ARM.Collect$$$$00000001) for _main_stk
    idiv.o(.text) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfb.o(i.__0fprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0fprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0printf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printfb.o(i.__0vfprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vfprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printf0.o(i.__0fprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0fprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0printf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf0.o(i.__0vfprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vfprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf1.o(i.__0fprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0fprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0printf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i.__0vfprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vfprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf2.o(i.__0fprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0fprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0printf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf2.o(i.__0vfprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vfprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf3.o(i.__0fprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0fprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0printf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i.__0vfprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vfprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf4.o(i.__0fprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0fprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0printf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i.__0vfprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vfprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf5.o(i.__0fprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0fprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0printf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i.__0vfprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vfprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf6.o(i.__0fprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0fprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0printf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i.__0vfprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vfprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i._printf_core) refers to printf6.o(i._printf_pre_padding) for _printf_pre_padding
    printf6.o(i._printf_core) refers to printf6.o(i._printf_post_padding) for _printf_post_padding
    printf6.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf7.o(i.__0fprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0fprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0printf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i.__0vfprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vfprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i._printf_core) refers to printf7.o(i._printf_pre_padding) for _printf_pre_padding
    printf7.o(i._printf_core) refers to printf7.o(i._printf_post_padding) for _printf_post_padding
    printf7.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf8.o(i.__0fprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0fprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0printf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i.__0vfprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vfprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i._printf_core) refers to printf8.o(i._printf_pre_padding) for _printf_pre_padding
    printf8.o(i._printf_core) refers to printf8.o(i._printf_post_padding) for _printf_post_padding
    printf8.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i.__0fprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0fprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0fprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0printf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0printf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0snprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0snprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0snprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0sprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0sprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0sprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i.__0vfprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vfprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vfprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0vsnprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0vsprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i._fp_digits) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._fp_digits) refers to dmul.o(.text) for __aeabi_dmul
    printfa.o(i._fp_digits) refers to ddiv.o(.text) for __aeabi_ddiv
    printfa.o(i._fp_digits) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    printfa.o(i._fp_digits) refers to dadd.o(.text) for __aeabi_dadd
    printfa.o(i._fp_digits) refers to dfixul.o(.text) for __aeabi_d2ulz
    printfa.o(i._fp_digits) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_core) refers to printfa.o(i._printf_pre_padding) for _printf_pre_padding
    printfa.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers to printfa.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i._printf_core) refers to printfa.o(i._fp_digits) for _fp_digits
    printfa.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfa.o(i._printf_post_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_pre_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._snputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._sputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    fmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers to fepilogue.o(.text) for _float_round
    fscalb.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    dadd.o(.text) refers to llsshr.o(.text) for __aeabi_lasr
    dadd.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dmul.o(.text) refers to depilogue.o(.text) for _double_epilogue
    fflti.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fflti.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    ffltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ffltui.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    dfltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfltui.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ffixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixui.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    f2d.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    d2f.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    d2f.o(.text) refers to fepilogue.o(.text) for _float_round
    cfcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    cfrcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    entry2.o(.ARM.Collect$$$$00000001) refers to entry2.o(.ARM.Collect$$$$00002712) for __lit__00000000
    entry2.o(.ARM.Collect$$$$00002712) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    entry5.o(.ARM.Collect$$$$00000004) refers to init.o(.text) for __scatterload
    entry9a.o(.ARM.Collect$$$$0000000B) refers to main.o(i.main) for main
    entry9b.o(.ARM.Collect$$$$0000000C) refers to main.o(i.main) for main
    uldiv.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    uldiv.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to depilogue.o(i.__ARM_clz) for __ARM_clz
    depilogue.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    ddiv.o(.text) refers to depilogue.o(.text) for _double_round
    dfixul.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixul.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    init.o(.text) refers to entry5.o(.ARM.Collect$$$$00000004) for __main_after_scatterload


==============================================================================

Removing Unused input sections from the image.

    Removing main.o(.rev16_text), (4 bytes).
    Removing main.o(.revsh_text), (4 bytes).
    Removing p6a_demo.o(.rev16_text), (4 bytes).
    Removing p6a_demo.o(.revsh_text), (4 bytes).
    Removing p6a_demo.o(i.Gpio_swire_output), (80 bytes).
    Removing p6a_demo.o(i.Panel_CCM), (42 bytes).
    Removing p6a_demo.o(i.ap_dcs_set_exit_idle_mode), (100 bytes).
    Removing p6a_demo.o(i.ap_dcs_set_frame_change), (52 bytes).
    Removing p6a_demo.o(i.ap_rstn_pull_down_cb), (88 bytes).
    Removing p6a_demo.o(i.ap_rstn_pull_high_cb), (28 bytes).
    Removing p6a_demo.o(i.ap_set_FPS_B1), (74 bytes).
    Removing p6a_demo.o(i.app_system_process), (108 bytes).
    Removing p6a_demo.o(i.app_system_resume), (64 bytes).
    Removing p6a_demo.o(i.app_system_suspend), (396 bytes).
    Removing p6a_demo.o(i.soft_te_timer_cb), (28 bytes).
    Removing p6a_demo.o(i.soft_te_timer_init), (40 bytes).
    Removing board.o(.rev16_text), (4 bytes).
    Removing board.o(.revsh_text), (4 bytes).
    Removing startup_armcm0.o(HEAP), (3072 bytes).
    Removing hal_dsi_rx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd), (220 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_short_cmd), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit), (148 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_line), (604 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init), (320 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern), (256 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_force_video_crtl), (12 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_cap_pixel_color), (10 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en), (8 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback), (52 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_write_cmd_entry), (10 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle), (40 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart), (68 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack), (176 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cap_pixel_pos), (10 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_check_crc), (24 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk), (32 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter), (44 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_log_level), (8 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data), (240 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data_ex), (392 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk), (72 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk), (56 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop), (48 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate), (10 bytes).
    Removing hal_dsi_rx_ctrl.o(i.swap_uint16_t), (10 bytes).
    Removing hal_dsi_tx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode), (112 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit), (116 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick), (244 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_frame), (12 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_get_disp_line), (12 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_overwrite_enable), (22 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_partial_disp_enable), (70 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd), (128 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle), (32 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs), (60 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm), (8 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_sync_line), (36 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect), (60 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance), (60 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness), (12 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div), (52 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc), (60 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg), (28 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop), (56 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera), (68 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update), (16 bytes).
    Removing hal_gpio.o(.rev16_text), (4 bytes).
    Removing hal_gpio.o(.revsh_text), (4 bytes).
    Removing hal_gpio.o(i.hal_gpio_ctrl_eint), (24 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_input_data), (18 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_int_type), (20 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_pull_state), (40 bytes).
    Removing hal_gpio.o(i.hal_gpio_init_eint), (64 bytes).
    Removing hal_gpio.o(i.hal_gpio_reg_eint_cb), (28 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_ap_reset_int), (80 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_driving_strength), (44 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_high_impedance), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_pull_state), (72 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_schmitt_trigger), (52 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_slew_rate), (52 bytes).
    Removing hal_system.o(.rev16_text), (4 bytes).
    Removing hal_system.o(.revsh_text), (4 bytes).
    Removing hal_system.o(i.hal_system_clear_debug_state), (10 bytes).
    Removing hal_system.o(i.hal_system_disable_systick), (8 bytes).
    Removing hal_system.o(i.hal_system_enable_systick), (8 bytes).
    Removing hal_system.o(i.hal_system_get_debug_state), (8 bytes).
    Removing hal_system.o(i.hal_system_get_tick), (8 bytes).
    Removing hal_system.o(i.hal_system_idle_mode), (8 bytes).
    Removing hal_system.o(i.hal_system_register_systick_cb), (8 bytes).
    Removing hal_system.o(i.hal_system_reset_chip), (10 bytes).
    Removing hal_timer.o(.rev16_text), (4 bytes).
    Removing hal_timer.o(.revsh_text), (4 bytes).
    Removing hal_timer.o(i.hal_timer_get_status), (8 bytes).
    Removing hal_timer.o(i.hal_timer_set_repeat), (8 bytes).
    Removing hal_timer.o(i.hal_timer_start_ex), (42 bytes).
    Removing hal_pwr.o(.rev16_text), (4 bytes).
    Removing hal_pwr.o(.revsh_text), (4 bytes).
    Removing hal_pwr.o(i.hal_pwr_elvcc_close), (10 bytes).
    Removing hal_pwr.o(i.hal_pwr_elvcc_ldo_en), (46 bytes).
    Removing hal_pwr.o(i.hal_pwr_elvcc_vol_set), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode), (42 bytes).
    Removing hal_pwr.o(i.hal_pwr_enter_normal_sleep_mode), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode), (100 bytes).
    Removing hal_pwr.o(i.hal_pwr_exit_sleep_mode), (10 bytes).
    Removing hal_pwr.o(i.hal_pwr_get_reset_flag), (66 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo13s_en), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo13s_set), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo18s_en), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo18s_set), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_set_pvd), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_set_sleep_mode_power), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin), (100 bytes).
    Removing hal_pwr.o(i.hal_pwr_set_vcc_enable), (8 bytes).
    Removing hal_pwr.o(i.stop_sleep_cb), (24 bytes).
    Removing hal_pwr.o(.data), (8 bytes).
    Removing tau_delay.o(.rev16_text), (4 bytes).
    Removing tau_delay.o(.revsh_text), (4 bytes).
    Removing tau_log.o(.rev16_text), (4 bytes).
    Removing tau_log.o(.revsh_text), (4 bytes).
    Removing tau_log.o(i.fgetc), (72 bytes).
    Removing hal_uart.o(.rev16_text), (4 bytes).
    Removing hal_uart.o(.revsh_text), (4 bytes).
    Removing hal_uart.o(i.hal_uart0_rx_dma_cb), (20 bytes).
    Removing hal_uart.o(i.hal_uart0_tx_dma_cb), (36 bytes).
    Removing hal_uart.o(i.hal_uart1_rx_dma_cb), (20 bytes).
    Removing hal_uart.o(i.hal_uart1_tx_dma_cb), (36 bytes).
    Removing hal_uart.o(i.hal_uart_deinit), (48 bytes).
    Removing hal_uart.o(i.hal_uart_dma_path_close), (92 bytes).
    Removing hal_uart.o(i.hal_uart_dma_recv), (276 bytes).
    Removing hal_uart.o(i.hal_uart_dma_send), (280 bytes).
    Removing hal_uart.o(i.hal_uart_recv_blocking), (28 bytes).
    Removing hal_uart.o(i.hal_uart_recv_none_blocking), (28 bytes).
    Removing hal_uart.o(i.hal_uart_send_none_blocking), (28 bytes).
    Removing hal_internal_vsync.o(.rev16_text), (4 bytes).
    Removing hal_internal_vsync.o(.revsh_text), (4 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te), (2 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_register_rx_callback), (28 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual), (28 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state), (12 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line), (60 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate), (134 bytes).
    Removing hal_internal_vsync.o(.data), (4 bytes).
    Removing hal_internal_dcs.o(.rev16_text), (4 bytes).
    Removing hal_internal_dcs.o(.revsh_text), (4 bytes).
    Removing hal_internal_dcs.o(i.hal_intl_dcs_register_write_cmd_entry), (12 bytes).
    Removing hal_internal_dcs.o(i.hal_intl_dcs_set_dcs_direct_mode), (44 bytes).
    Removing hal_internal_fb.o(.rev16_text), (4 bytes).
    Removing hal_internal_fb.o(.revsh_text), (4 bytes).
    Removing hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual), (480 bytes).
    Removing hal_internal_fb.o(.conststring), (152 bytes).
    Removing hal_internal_svs.o(.rev16_text), (4 bytes).
    Removing hal_internal_svs.o(.revsh_text), (4 bytes).
    Removing hal_internal_svs.o(i.hal_intl_svs_set_input_frate), (112 bytes).
    Removing hal_internal_svs.o(i.hal_intl_svs_set_sync_coef), (12 bytes).
    Removing drv_common.o(.rev16_text), (4 bytes).
    Removing drv_common.o(.revsh_text), (4 bytes).
    Removing drv_common.o(i.drv_common_disable_systick), (20 bytes).
    Removing drv_common.o(i.drv_common_enable_systick), (88 bytes).
    Removing drv_common.o(i.drv_common_get_tick), (12 bytes).
    Removing drv_common.o(i.drv_common_idle_mode), (40 bytes).
    Removing drv_common.o(i.drv_common_systick_register_cb), (12 bytes).
    Removing drv_crgu.o(.rev16_text), (4 bytes).
    Removing drv_crgu.o(.revsh_text), (4 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_all_reset_flags), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_reset_flag), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_all_reset_flag), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_reset_flag), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_system_clk), (104 bytes).
    Removing drv_crgu.o(i.drv_crgu_reset_chip), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_reset_modules), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_clock_div), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_clock_src), (16 bytes).
    Removing drv_dsc_dec.o(.rev16_text), (4 bytes).
    Removing drv_dsc_dec.o(.revsh_text), (4 bytes).
    Removing drv_dsc_dec.o(i.drv_dsc_dec_disable), (28 bytes).
    Removing drv_gpio.o(.rev16_text), (4 bytes).
    Removing drv_gpio.o(.revsh_text), (4 bytes).
    Removing drv_gpio.o(i.drv_gpio_get_attribute), (16 bytes).
    Removing drv_gpio.o(i.drv_gpio_get_input_data), (24 bytes).
    Removing drv_gpio.o(i.drv_gpio_register_ap_reset_callback), (12 bytes).
    Removing drv_gpio.o(i.drv_gpio_register_callback), (20 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_attribute), (28 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_int), (68 bytes).
    Removing drv_pwr.o(.rev16_text), (4 bytes).
    Removing drv_pwr.o(.revsh_text), (4 bytes).
    Removing drv_pwr.o(i.drv_pwr_10bit_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_analog_pwm_en), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_charge_pump_en), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_close_iov18_tp18), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_dsc_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_elvcc_pwm_en), (124 bytes).
    Removing drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode), (76 bytes).
    Removing drv_pwr.o(i.drv_pwr_enter_sleep_mode), (152 bytes).
    Removing drv_pwr.o(i.drv_pwr_enter_sleep_mode_ex), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_enter_stop_sleep_mode), (152 bytes).
    Removing drv_pwr.o(i.drv_pwr_exit_sleep_mode), (40 bytes).
    Removing drv_pwr.o(i.drv_pwr_exit_sleep_mode_ex), (40 bytes).
    Removing drv_pwr.o(i.drv_pwr_fb_pd), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_get_wakeflag), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_get_write_lock_st), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_hf_frm_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_10M_clock), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_mode_clock_sel), (60 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_mode_sel), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_voltage_set), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo11d_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo13s_en), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo13s_set), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo15_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo18s_en), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo18s_set), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_ltpo_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_osc32k_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_osc80m_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_p3k_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_por_mode_flag), (32 bytes).
    Removing drv_pwr.o(i.drv_pwr_power_in), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_power_ready_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_power_sel), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwm_output_pwm_led), (56 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_driver_current_Big_step), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_driver_current_small_step), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_electric_current), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_open_drain), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_ram_pd_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_read_boot_chipst), (12 bytes).
    Removing drv_pwr.o(i.drv_pwr_read_chipcfg), (12 bytes).
    Removing drv_pwr.o(i.drv_pwr_rgbr_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_ap_rst_mode), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_breath_screen_power_sel), (40 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_ldo11_mode), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_ldo15_mode), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_pvd), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_pvd_mode), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_system_clk), (32 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_wakeup_type), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_sw_tp18_en), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_wakeflag_get), (16 bytes).
    Removing drv_sys_cfg.o(.rev16_text), (4 bytes).
    Removing drv_sys_cfg.o(.revsh_text), (4 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig), (36 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_sel_dma_req), (128 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group), (36 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig), (36 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_sel_swire_timer), (24 bytes).
    Removing drv_timer.o(.rev16_text), (4 bytes).
    Removing drv_timer.o(.revsh_text), (4 bytes).
    Removing drv_timer.o(i.drv_timer_get_status), (38 bytes).
    Removing dcs_packet_fifo.o(.rev16_text), (4 bytes).
    Removing dcs_packet_fifo.o(.revsh_text), (4 bytes).
    Removing dcs_packet_fifo.o(i.dcs_packet_get_fifo_size), (16 bytes).
    Removing drv_se.o(.rev16_text), (4 bytes).
    Removing drv_se.o(.revsh_text), (4 bytes).
    Removing drv_dsi_rx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_rx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_force_video_crtl), (28 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_lpdt_fifo_status), (16 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate), (68 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_version), (12 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg), (24 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_drv_log_level), (12 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg), (48 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_shut_down), (24 bytes).
    Removing drv_dsi_tx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_tx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_force_interrupt), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_get_phy_status), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_forcepll), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_start), (24 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot), (68 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger), (92 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter), (296 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit), (228 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_sdf_3d), (32 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_bta), (28 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_vpg), (100 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_version), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_vid_shadow), (20 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_clear), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_lock), (32 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_read), (16 bytes).
    Removing drv_lcdc.o(.rev16_text), (4 bytes).
    Removing drv_lcdc.o(.revsh_text), (4 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_clear_irq), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_dpisignal_output_ctrl), (44 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_fixed_frame_output), (56 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_dpbuf_num), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_dpi_status), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_frame_clk_count), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_int_en_status), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_int_status), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_line_status), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_rgb2pen_subpixel), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_part_display_config), (52 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_pixel_value_config), (32 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_rd_st_line_config), (28 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_software_reset), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_stop_display), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_update_shadow_reg), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_vid_sw_start), (56 bytes).
    Removing drv_memc.o(.rev16_text), (4 bytes).
    Removing drv_memc.o(.revsh_text), (4 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_frm_time), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_int_frame), (36 bytes).
    Removing drv_memc.o(i.drv_memc_set_double_buffer_reverse), (24 bytes).
    Removing drv_memc.o(i.drv_memc_set_fb_pri), (44 bytes).
    Removing drv_memc.o(i.drv_memc_set_fb_remaining_line_trigger), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_inten), (28 bytes).
    Removing drv_memc.o(i.drv_memc_set_read_trigger_line), (24 bytes).
    Removing drv_memc.o(i.drv_memc_set_te_ind), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_tear_hwclr), (24 bytes).
    Removing drv_memc.o(i.drv_memc_set_vidc_fb_arb), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_write_trigger_line), (24 bytes).
    Removing drv_rxbr.o(.rev16_text), (4 bytes).
    Removing drv_rxbr.o(.revsh_text), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_clr_swp_cnt), (16 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_dsc_flush), (24 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_col_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_cur_hline_rcv_cnt), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_frame_data_interval), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_hline_dcat), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_ipi_vsync_interval), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_page_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_pix_fmt), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_swpxl_cnt), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg), (20 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_register_irq0_callback), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_ack_pkt_md), (28 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_cmd_filter), (320 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_cmd_response), (324 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_col_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_compress), (32 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_data_catch_hline), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_page_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_swpxl_data), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_tmpdith_bp), (28 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_soft_reset), (32 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_sw_reset), (164 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_swpxl_clr), (32 bytes).
    Removing drv_vidc.o(.rev16_text), (4 bytes).
    Removing drv_vidc.o(.revsh_text), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_clear_status0), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_cap_pixel), (28 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_signal_frame), (36 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status0), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status1), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status2), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_dsc_thresh), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_frmst_latency), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_inff_thresh), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_irq_line), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_module_enable), (28 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_outff_thresh), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_update_src_format), (20 bytes).
    Removing drv_dma.o(.rev16_text), (4 bytes).
    Removing drv_dma.o(.revsh_text), (4 bytes).
    Removing drv_dma.o(i.drv_dma_apply_handle), (304 bytes).
    Removing drv_dma.o(i.drv_dma_deinit), (52 bytes).
    Removing drv_dma.o(i.drv_dma_disable), (20 bytes).
    Removing drv_dma.o(i.drv_dma_disable_int), (40 bytes).
    Removing drv_dma.o(i.drv_dma_enable), (36 bytes).
    Removing drv_dma.o(i.drv_dma_enable_int), (68 bytes).
    Removing drv_dma.o(i.drv_dma_get_remaining_trans_num), (20 bytes).
    Removing drv_dma.o(i.drv_dma_get_status), (20 bytes).
    Removing drv_dma.o(i.drv_dma_init), (22 bytes).
    Removing drv_dma.o(i.drv_dma_int_list_delete), (88 bytes).
    Removing drv_dma.o(i.drv_dma_int_list_inset), (48 bytes).
    Removing drv_dma.o(i.drv_dma_register_callback), (4 bytes).
    Removing drv_dma.o(i.drv_dma_reset), (36 bytes).
    Removing drv_dma.o(i.drv_dma_set_bitwide), (56 bytes).
    Removing drv_dma.o(i.drv_dma_set_burst), (20 bytes).
    Removing drv_dma.o(i.drv_dma_set_circle_mode), (40 bytes).
    Removing drv_dma.o(i.drv_dma_set_dir), (40 bytes).
    Removing drv_dma.o(i.drv_dma_set_increment), (72 bytes).
    Removing drv_dma.o(i.drv_dma_set_mem_trans_info), (40 bytes).
    Removing drv_dma.o(i.drv_dma_set_mem_trans_offset), (24 bytes).
    Removing drv_dma.o(i.drv_dma_set_per_address), (20 bytes).
    Removing drv_dma.o(i.drv_dma_set_priority), (32 bytes).
    Removing drv_dma.o(i.drv_dma_set_tran_int_cnt), (28 bytes).
    Removing drv_dma.o(i.drv_dma_update_handle_setting), (148 bytes).
    Removing drv_dma.o(i.drv_dma_update_req_by_default), (40 bytes).
    Removing drv_dma.o(.constdata), (136 bytes).
    Removing drv_uart.o(.rev16_text), (4 bytes).
    Removing drv_uart.o(.revsh_text), (4 bytes).
    Removing drv_uart.o(i.drv_uart_deinit), (60 bytes).
    Removing drv_uart.o(i.drv_uart_get_def_cfg), (72 bytes).
    Removing drv_uart.o(i.drv_uart_recv_blocking), (48 bytes).
    Removing drv_uart.o(i.drv_uart_recv_none_blocking), (60 bytes).
    Removing drv_uart.o(i.drv_uart_send_none_blocking), (60 bytes).
    Removing drv_efuse.o(.rev16_text), (4 bytes).
    Removing drv_efuse.o(.revsh_text), (4 bytes).
    Removing drv_efuse.o(i.drv_efuse_crc_cal), (128 bytes).
    Removing drv_efuse.o(i.drv_efuse_get_default_config), (26 bytes).
    Removing drv_efuse.o(i.drv_efuse_int_disable), (12 bytes).
    Removing drv_efuse.o(i.drv_efuse_write), (56 bytes).
    Removing drv_efuse.o(i.drv_efuse_write_read_req_clear), (22 bytes).
    Removing drv_efuse.o(i.drv_efuse_write_req), (22 bytes).
    Removing drv_phy_common.o(.rev16_text), (4 bytes).
    Removing drv_phy_common.o(.revsh_text), (4 bytes).
    Removing drv_per_common.o(.rev16_text), (4 bytes).
    Removing drv_per_common.o(.revsh_text), (4 bytes).
    Removing drv_per_common.o(i.drv_per_get_system_clk), (8 bytes).
    Removing drv_per_common.o(i.drv_per_reset_module), (14 bytes).
    Removing drv_per_common.o(i.drv_per_set_clock), (14 bytes).
    Removing fflti.o(.text), (22 bytes).

412 unused section(s) (total 20616 bytes) removed from the image.

==============================================================================

Image Symbol Table

    Local Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    ../clib/../cmprslib/zerorunl2.c          0x00000000   Number         0  __dczerorl2.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uidiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uldiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  idiv.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry5.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry2.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9a.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llsshr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llushr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llshl.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf1.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfb.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf6.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf2.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf3.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf0.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf4.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf5.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf7.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf8.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfa.o ABSOLUTE
    ../clib/microlib/printf/stubs.s          0x00000000   Number         0  stubs.o ABSOLUTE
    ../clib/microlib/stdio/streams.c         0x00000000   Number         0  stdout.o ABSOLUTE
    ../clib/microlib/string/memcmp.c         0x00000000   Number         0  memcmp.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpyb.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpya.o ABSOLUTE
    ../clib/microlib/string/memset.c         0x00000000   Number         0  memseta.o ABSOLUTE
    ../clib/microlib/string/strlen.c         0x00000000   Number         0  strlen.o ABSOLUTE
    ../clib/microlib/stubs.s                 0x00000000   Number         0  iusefp.o ABSOLUTE
    ../fplib/microlib/d2f.c                  0x00000000   Number         0  d2f.o ABSOLUTE
    ../fplib/microlib/f2d.c                  0x00000000   Number         0  f2d.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  dadd.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  fadd.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  fdiv.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  ddiv.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  fepilogue.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  depilogue.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  ffixui.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixui.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixul.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  ffltui.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  fflti.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  dfltui.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  dmul.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  fmul.o ABSOLUTE
    ../fplib/microlib/fpscalb.c              0x00000000   Number         0  fscalb.o ABSOLUTE
    ../mathlib/ceil.c                        0x00000000   Number         0  ceil.o ABSOLUTE
    ..\..\..\src\common\tau_delay.c          0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\..\..\src\common\tau_log.c            0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_per_common.c 0x00000000   Number         0  drv_per_common.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_pwr.c 0x00000000   Number         0  hal_pwr.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_timer.c 0x00000000   Number         0  hal_timer.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\dcs_packet_fifo.c 0x00000000   Number         0  dcs_packet_fifo.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_dcs.c 0x00000000   Number         0  hal_internal_dcs.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_fb.c 0x00000000   Number         0  hal_internal_fb.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_svs.c 0x00000000   Number         0  hal_internal_svs.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\src\drv_se.c  0x00000000   Number         0  drv_se.o ABSOLUTE
    ..\..\src\app\P6A\p6a_demo.c             0x00000000   Number         0  p6a_demo.o ABSOLUTE
    ..\..\src\app\main.c                     0x00000000   Number         0  main.o ABSOLUTE
    ..\..\src\board\board.c                  0x00000000   Number         0  board.o ABSOLUTE
    ..\..\src\board\startup\startup_ARMCM0.s 0x00000000   Number         0  startup_armcm0.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_delay.c     0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_log.c       0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_per_common.c 0x00000000   Number         0  drv_per_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_pwr.c 0x00000000   Number         0  hal_pwr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_timer.c 0x00000000   Number         0  hal_timer.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\dcs_packet_fifo.c 0x00000000   Number         0  dcs_packet_fifo.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_dcs.c 0x00000000   Number         0  hal_internal_dcs.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_fb.c 0x00000000   Number         0  hal_internal_fb.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_svs.c 0x00000000   Number         0  hal_internal_svs.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\src\\drv_se.c 0x00000000   Number         0  drv_se.o ABSOLUTE
    ..\\..\\src\\app\\P6A\\p6a_demo.c        0x00000000   Number         0  p6a_demo.o ABSOLUTE
    ..\\..\\src\\app\\main.c                 0x00000000   Number         0  main.o ABSOLUTE
    ..\\..\\src\\board\\board.c              0x00000000   Number         0  board.o ABSOLUTE
    cdrcmple.s                               0x00000000   Number         0  cdrcmple.o ABSOLUTE
    cfcmple.s                                0x00000000   Number         0  cfcmple.o ABSOLUTE
    cfrcmple.s                               0x00000000   Number         0  cfrcmple.o ABSOLUTE
    dc.s                                     0x00000000   Number         0  dc.o ABSOLUTE
    handlers.s                               0x00000000   Number         0  handlers.o ABSOLUTE
    init.s                                   0x00000000   Number         0  init.o ABSOLUTE
    RESET                                    0x00010000   Section      192  startup_armcm0.o(RESET)
    .ARM.Collect$$$$00000000                 0x000100c0   Section        0  entry.o(.ARM.Collect$$$$00000000)
    .ARM.Collect$$$$00000001                 0x000100c0   Section        4  entry2.o(.ARM.Collect$$$$00000001)
    .ARM.Collect$$$$00000004                 0x000100c4   Section        4  entry5.o(.ARM.Collect$$$$00000004)
    .ARM.Collect$$$$00000008                 0x000100c8   Section        0  entry7b.o(.ARM.Collect$$$$00000008)
    .ARM.Collect$$$$0000000A                 0x000100c8   Section        0  entry8b.o(.ARM.Collect$$$$0000000A)
    .ARM.Collect$$$$0000000B                 0x000100c8   Section        8  entry9a.o(.ARM.Collect$$$$0000000B)
    .ARM.Collect$$$$0000000D                 0x000100d0   Section        0  entry10a.o(.ARM.Collect$$$$0000000D)
    .ARM.Collect$$$$0000000F                 0x000100d0   Section        0  entry11a.o(.ARM.Collect$$$$0000000F)
    .ARM.Collect$$$$00002712                 0x000100d0   Section        4  entry2.o(.ARM.Collect$$$$00002712)
    __lit__00000000                          0x000100d0   Data           4  entry2.o(.ARM.Collect$$$$00002712)
    .text                                    0x000100d4   Section      120  startup_armcm0.o(.text)
    .text                                    0x0001014c   Section        0  uidiv.o(.text)
    .text                                    0x00010178   Section        0  idiv.o(.text)
    .text                                    0x000101a0   Section        0  memcpya.o(.text)
    .text                                    0x000101c4   Section        0  memseta.o(.text)
    .text                                    0x000101e8   Section        0  strlen.o(.text)
    .text                                    0x000101f6   Section        0  memcmp.o(.text)
    .text                                    0x00010210   Section        0  fadd.o(.text)
    .text                                    0x000102c2   Section        0  fmul.o(.text)
    .text                                    0x0001033c   Section        0  fdiv.o(.text)
    .text                                    0x000103b8   Section        0  fscalb.o(.text)
    .text                                    0x000103d0   Section        0  dadd.o(.text)
    .text                                    0x00010534   Section        0  dmul.o(.text)
    .text                                    0x00010604   Section        0  ffltui.o(.text)
    .text                                    0x00010614   Section        0  dfltui.o(.text)
    .text                                    0x00010630   Section        0  ffixui.o(.text)
    .text                                    0x00010658   Section        0  dfixui.o(.text)
    .text                                    0x00010694   Section        0  f2d.o(.text)
    .text                                    0x000106bc   Section        0  d2f.o(.text)
    .text                                    0x000106f4   Section       20  cfcmple.o(.text)
    .text                                    0x00010708   Section       20  cfrcmple.o(.text)
    .text                                    0x0001071c   Section        0  uldiv.o(.text)
    .text                                    0x0001077c   Section        0  llshl.o(.text)
    .text                                    0x0001079c   Section        0  llushr.o(.text)
    .text                                    0x000107be   Section        0  llsshr.o(.text)
    .text                                    0x000107e4   Section        0  iusefp.o(.text)
    .text                                    0x000107e4   Section        0  fepilogue.o(.text)
    .text                                    0x00010866   Section        0  depilogue.o(.text)
    .text                                    0x00010924   Section        0  ddiv.o(.text)
    .text                                    0x00010a14   Section        0  dfixul.o(.text)
    .text                                    0x00010a54   Section       40  cdrcmple.o(.text)
    .text                                    0x00010a7c   Section       36  init.o(.text)
    .text                                    0x00010aa0   Section        0  __dczerorl2.o(.text)
    i.AP_NRESET_IRQn_Handler                 0x00010af8   Section        0  drv_gpio.o(i.AP_NRESET_IRQn_Handler)
    i.DMA_IRQn_Handler                       0x00010b14   Section        0  drv_dma.o(i.DMA_IRQn_Handler)
    i.EXTI_INT0_IRQn_Handler                 0x00010b70   Section        0  drv_gpio.o(i.EXTI_INT0_IRQn_Handler)
    i.EXTI_INT1_IRQn_Handler                 0x00010b7a   Section        0  drv_gpio.o(i.EXTI_INT1_IRQn_Handler)
    i.EXTI_INT2_IRQn_Handler                 0x00010b84   Section        0  drv_gpio.o(i.EXTI_INT2_IRQn_Handler)
    i.EXTI_INT3_IRQn_Handler                 0x00010b8e   Section        0  drv_gpio.o(i.EXTI_INT3_IRQn_Handler)
    i.EXTI_INT4_IRQn_Handler                 0x00010b98   Section        0  drv_gpio.o(i.EXTI_INT4_IRQn_Handler)
    i.EXTI_INT5_IRQn_Handler                 0x00010ba2   Section        0  drv_gpio.o(i.EXTI_INT5_IRQn_Handler)
    i.EXTI_INT6_IRQn_Handler                 0x00010bac   Section        0  drv_gpio.o(i.EXTI_INT6_IRQn_Handler)
    i.EXTI_INT7_IRQn_Handler                 0x00010bb6   Section        0  drv_gpio.o(i.EXTI_INT7_IRQn_Handler)
    i.HardFault_Handler                      0x00010bc0   Section        0  drv_common.o(i.HardFault_Handler)
    i.LCDC_IRQn_Handler                      0x00010c08   Section        0  hal_internal_vsync.o(i.LCDC_IRQn_Handler)
    i.MEMC_IRQn_Handler                      0x00010d08   Section        0  drv_memc.o(i.MEMC_IRQn_Handler)
    i.MIPI_TX_IRQn_Handler                   0x00010da4   Section        0  drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler)
    i.SysTick_Handler                        0x00010e5c   Section        0  drv_common.o(i.SysTick_Handler)
    i.TIMER0_IRQn_Handler                    0x00010e74   Section        0  drv_timer.o(i.TIMER0_IRQn_Handler)
    i.TIMER1_IRQn_Handler                    0x00010e7e   Section        0  drv_timer.o(i.TIMER1_IRQn_Handler)
    i.TIMER2_IRQn_Handler                    0x00010e88   Section        0  drv_timer.o(i.TIMER2_IRQn_Handler)
    i.TIMER3_IRQn_Handler                    0x00010e92   Section        0  drv_timer.o(i.TIMER3_IRQn_Handler)
    i.VIDC_IRQn_Handler                      0x00010e9c   Section        0  drv_vidc.o(i.VIDC_IRQn_Handler)
    i.VPRE1_IRQn_Handler                     0x00010eb8   Section        0  drv_rxbr.o(i.VPRE1_IRQn_Handler)
    i.VPRE_IRQn_Handler                      0x00010ed4   Section        0  hal_internal_dcs.o(i.VPRE_IRQn_Handler)
    i.__0printf                              0x00010f40   Section        0  printfa.o(i.__0printf)
    i.__0vsprintf                            0x00010f60   Section        0  printfa.o(i.__0vsprintf)
    i.__ARM_clz                              0x00010f84   Section        0  depilogue.o(i.__ARM_clz)
    i.__ARM_common_switch8                   0x00010fb2   Section        0  hal_dsi_rx_ctrl.o(i.__ARM_common_switch8)
    i.__NVIC_DisableIRQ                      0x00010fcc   Section        0  drv_rxbr.o(i.__NVIC_DisableIRQ)
    __NVIC_DisableIRQ                        0x00010fcd   Thumb Code    26  drv_rxbr.o(i.__NVIC_DisableIRQ)
    i.__scatterload_copy                     0x00010fec   Section       14  handlers.o(i.__scatterload_copy)
    i.__scatterload_null                     0x00010ffa   Section        2  handlers.o(i.__scatterload_null)
    .ARM.__at_0x11000                        0x00011000   Section       28  drv_common.o(.ARM.__at_0x11000)
    .ARM.__at_0x1101C                        0x0001101c   Section       16  tau_log.o(.ARM.__at_0x1101C)
    .ARM.__at_0x1102C                        0x0001102c   Section       22  hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C)
    i.MIPI_RX_IRQn_Handler                   0x00011044   Section        0  drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler)
    i.UART_IRQn_Handler                      0x000113a8   Section        0  drv_uart.o(i.UART_IRQn_Handler)
    i.__NVIC_EnableIRQ                       0x00011528   Section        0  drv_rxbr.o(i.__NVIC_EnableIRQ)
    __NVIC_EnableIRQ                         0x00011529   Thumb Code    18  drv_rxbr.o(i.__NVIC_EnableIRQ)
    i.__scatterload_zeroinit                 0x00011540   Section       14  handlers.o(i.__scatterload_zeroinit)
    i._fp_digits                             0x00011550   Section        0  printfa.o(i._fp_digits)
    _fp_digits                               0x00011551   Thumb Code   344  printfa.o(i._fp_digits)
    i._printf_core                           0x000116c4   Section        0  printfa.o(i._printf_core)
    _printf_core                             0x000116c5   Thumb Code  1754  printfa.o(i._printf_core)
    i._printf_post_padding                   0x00011db0   Section        0  printfa.o(i._printf_post_padding)
    _printf_post_padding                     0x00011db1   Thumb Code    32  printfa.o(i._printf_post_padding)
    i._printf_pre_padding                    0x00011dd0   Section        0  printfa.o(i._printf_pre_padding)
    _printf_pre_padding                      0x00011dd1   Thumb Code    44  printfa.o(i._printf_pre_padding)
    i._sputc                                 0x00011dfc   Section        0  printfa.o(i._sputc)
    _sputc                                   0x00011dfd   Thumb Code    10  printfa.o(i._sputc)
    i.ap_dcs_read                            0x00011e08   Section        0  p6a_demo.o(i.ap_dcs_read)
    ap_dcs_read                              0x00011e09   Thumb Code   280  p6a_demo.o(i.ap_dcs_read)
    i.ap_dcs_set_backlight                   0x00011f4c   Section        0  p6a_demo.o(i.ap_dcs_set_backlight)
    ap_dcs_set_backlight                     0x00011f4d   Thumb Code   146  p6a_demo.o(i.ap_dcs_set_backlight)
    i.ap_dcs_set_display_off                 0x00011ff0   Section        0  p6a_demo.o(i.ap_dcs_set_display_off)
    ap_dcs_set_display_off                   0x00011ff1   Thumb Code    34  p6a_demo.o(i.ap_dcs_set_display_off)
    i.ap_dcs_set_display_on                  0x00012038   Section        0  p6a_demo.o(i.ap_dcs_set_display_on)
    ap_dcs_set_display_on                    0x00012039   Thumb Code    40  p6a_demo.o(i.ap_dcs_set_display_on)
    i.ap_dcs_set_enter_sleep_mode            0x0001207c   Section        0  p6a_demo.o(i.ap_dcs_set_enter_sleep_mode)
    ap_dcs_set_enter_sleep_mode              0x0001207d   Thumb Code    90  p6a_demo.o(i.ap_dcs_set_enter_sleep_mode)
    i.ap_dcs_set_exit_sleep_mode             0x000120dc   Section        0  p6a_demo.o(i.ap_dcs_set_exit_sleep_mode)
    ap_dcs_set_exit_sleep_mode               0x000120dd   Thumb Code    28  p6a_demo.o(i.ap_dcs_set_exit_sleep_mode)
    i.app_display_init                       0x0001211c   Section        0  p6a_demo.o(i.app_display_init)
    i.app_gpio_init                          0x0001213c   Section        0  p6a_demo.o(i.app_gpio_init)
    i.app_init_panel                         0x00012158   Section        0  p6a_demo.o(i.app_init_panel)
    app_init_panel                           0x00012159   Thumb Code    16  p6a_demo.o(i.app_init_panel)
    i.app_mipi_rx_init                       0x00012170   Section        0  p6a_demo.o(i.app_mipi_rx_init)
    app_mipi_rx_init                         0x00012171   Thumb Code   238  p6a_demo.o(i.app_mipi_rx_init)
    i.app_mipi_tx_init                       0x0001229c   Section        0  p6a_demo.o(i.app_mipi_tx_init)
    app_mipi_tx_init                         0x0001229d   Thumb Code   202  p6a_demo.o(i.app_mipi_tx_init)
    i.app_mipi_tx_start                      0x00012394   Section        0  p6a_demo.o(i.app_mipi_tx_start)
    app_mipi_tx_start                        0x00012395   Thumb Code    98  p6a_demo.o(i.app_mipi_tx_start)
    i.app_tx_panel_reset                     0x00012420   Section        0  p6a_demo.o(i.app_tx_panel_reset)
    app_tx_panel_reset                       0x00012421   Thumb Code    46  p6a_demo.o(i.app_tx_panel_reset)
    i.board_Init                             0x00012450   Section        0  board.o(i.board_Init)
    i.ceil                                   0x00012468   Section        0  ceil.o(i.ceil)
    i.check_mipi_rx_tx_video_info            0x00012530   Section        0  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    check_mipi_rx_tx_video_info              0x00012531   Thumb Code    44  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    i.check_pkt_buf_rev                      0x0001255c   Section        0  hal_internal_dcs.o(i.check_pkt_buf_rev)
    check_pkt_buf_rev                        0x0001255d   Thumb Code    84  hal_internal_dcs.o(i.check_pkt_buf_rev)
    i.dcs_packet_fifo_alloc                  0x000125e4   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    i.dcs_packet_fifo_init                   0x0001263c   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    i.dcs_packet_free_fifo_header            0x00012654   Section        0  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    i.dcs_packet_get_fifo_header             0x00012698   Section        0  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    i.delayMs                                0x000126bc   Section        0  tau_delay.o(i.delayMs)
    i.delayUs                                0x000126d4   Section        0  tau_delay.o(i.delayUs)
    i.drv_common_system_init                 0x00012700   Section        0  drv_common.o(i.drv_common_system_init)
    i.drv_crgu_enable_clock                  0x00012708   Section        0  drv_crgu.o(i.drv_crgu_enable_clock)
    i.drv_crgu_get_rxbr_clk                  0x00012744   Section        0  drv_crgu.o(i.drv_crgu_get_rxbr_clk)
    i.drv_crgu_set_ahb_clk                   0x000127ac   Section        0  drv_crgu.o(i.drv_crgu_set_ahb_clk)
    i.drv_crgu_set_dpi_clk                   0x000127d4   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_clk)
    i.drv_crgu_set_dsc_clk                   0x00012810   Section        0  drv_crgu.o(i.drv_crgu_set_dsc_clk)
    i.drv_crgu_set_fb_clk                    0x00012848   Section        0  drv_crgu.o(i.drv_crgu_set_fb_clk)
    i.drv_crgu_set_lcdc_clk                  0x00012870   Section        0  drv_crgu.o(i.drv_crgu_set_lcdc_clk)
    i.drv_crgu_set_reset                     0x00012898   Section        0  drv_crgu.o(i.drv_crgu_set_reset)
    i.drv_crgu_set_rxbr_clk                  0x000128b0   Section        0  drv_crgu.o(i.drv_crgu_set_rxbr_clk)
    i.drv_crgu_set_vidc_clk                  0x000128d8   Section        0  drv_crgu.o(i.drv_crgu_set_vidc_clk)
    i.drv_dma_clear_status                   0x00012900   Section        0  drv_dma.o(i.drv_dma_clear_status)
    i.drv_dma_get_int_source                 0x00012918   Section        0  drv_dma.o(i.drv_dma_get_int_source)
    drv_dma_get_int_source                   0x00012919   Thumb Code    16  drv_dma.o(i.drv_dma_get_int_source)
    i.drv_dsc_dec_enable                     0x0001292c   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    i.drv_dsc_dec_get_nslc                   0x00012964   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    i.drv_dsc_dec_set_irqen                  0x00012984   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_set_irqen)
    i.drv_dsi_rx_calc_ipi_tx_delay           0x000129a0   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    i.drv_dsi_rx_enable_irq                  0x00012aac   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    i.drv_dsi_rx_get_color_bpp               0x00012aec   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    drv_dsi_rx_get_color_bpp                 0x00012aed   Thumb Code    62  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    i.drv_dsi_rx_get_color_pcc               0x00012b3c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    drv_dsi_rx_get_color_pcc                 0x00012b3d   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    i.drv_dsi_rx_get_compression_en          0x00012b58   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    i.drv_dsi_rx_get_ddi_crc_en              0x00012b68   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_ddi_crc_en)
    i.drv_dsi_rx_get_max_ret_size            0x00012b78   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size)
    i.drv_dsi_rx_power_up                    0x00012b84   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    i.drv_dsi_rx_set_check_crc               0x00012b9c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc)
    i.drv_dsi_rx_set_ctrl_cfg                0x00012bb8   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    i.drv_dsi_rx_set_ddi_cfg                 0x00012bdc   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    i.drv_dsi_rx_set_ddi_crc_en              0x00012bec   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_crc_en)
    i.drv_dsi_rx_set_inten                   0x00012c08   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    i.drv_dsi_rx_set_ipi_cfg                 0x00012c14   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    i.drv_dsi_rx_set_ipi_ycbcr_frmt          0x00012c24   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_ycbcr_frmt)
    i.drv_dsi_rx_set_lane_swap               0x00012c40   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    i.drv_dsi_rx_set_resp_cnt                0x00012c54   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    i.drv_dsi_rx_set_tear_resp_en            0x00012c78   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_tear_resp_en)
    i.drv_dsi_rx_set_up_phy                  0x00012c94   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    i.drv_dsi_tx_command_header              0x00012d94   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    i.drv_dsi_tx_command_mode_cfg            0x00012dac   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    i.drv_dsi_tx_command_put_payload         0x00012e04   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    i.drv_dsi_tx_config_eotp                 0x00012e10   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    i.drv_dsi_tx_config_int                  0x00012e30   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    i.drv_dsi_tx_dpi_lpcmd_time              0x00012e3c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    i.drv_dsi_tx_dpi_mode                    0x00012e4c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    i.drv_dsi_tx_dpi_polarity                0x00012e5c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    i.drv_dsi_tx_edpi_cmd_size               0x00012e80   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    i.drv_dsi_tx_get_cmd_status              0x00012e8c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    i.drv_dsi_tx_mode                        0x00012e98   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    i.drv_dsi_tx_phy_clock_lane_auto_lp      0x00012ea4   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    i.drv_dsi_tx_phy_clock_lane_req_hs       0x00012ec0   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    i.drv_dsi_tx_phy_lane_mode               0x00012ee0   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    i.drv_dsi_tx_phy_status_ready            0x00012ef0   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    i.drv_dsi_tx_phy_status_stopstate        0x00012f58   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    i.drv_dsi_tx_phy_test_setup              0x00012f9c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    i.drv_dsi_tx_phy_time_cfg                0x000130ec   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    i.drv_dsi_tx_powerup                     0x0001310c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    i.drv_dsi_tx_response_mode               0x00013118   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    i.drv_dsi_tx_set_bta_ack                 0x0001313c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    i.drv_dsi_tx_set_esc_div                 0x00013158   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    i.drv_dsi_tx_set_int                     0x0001316c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    i.drv_dsi_tx_set_time_out_div            0x000131ac   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    i.drv_dsi_tx_set_video_chunk             0x000131c4   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    i.drv_dsi_tx_set_video_timing            0x000131d8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    i.drv_dsi_tx_shutdown                    0x000131fc   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    i.drv_dsi_tx_timeout_cfg                 0x00013208   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    i.drv_dsi_tx_video_mode_cfg              0x00013234   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    i.drv_efuse_enter_inactive               0x0001331c   Section        0  drv_efuse.o(i.drv_efuse_enter_inactive)
    i.drv_efuse_int_enable                   0x00013352   Section        0  drv_efuse.o(i.drv_efuse_int_enable)
    i.drv_efuse_read                         0x0001335e   Section        0  drv_efuse.o(i.drv_efuse_read)
    i.drv_efuse_read_req                     0x00013398   Section        0  drv_efuse.o(i.drv_efuse_read_req)
    i.drv_gpio_handle_int                    0x000133b0   Section        0  drv_gpio.o(i.drv_gpio_handle_int)
    drv_gpio_handle_int                      0x000133b1   Thumb Code    30  drv_gpio.o(i.drv_gpio_handle_int)
    i.drv_gpio_set_ioe                       0x000133d4   Section        0  drv_gpio.o(i.drv_gpio_set_ioe)
    i.drv_gpio_set_mode                      0x000133f4   Section        0  drv_gpio.o(i.drv_gpio_set_mode)
    i.drv_gpio_set_output_data               0x00013408   Section        0  hal_gpio.o(i.drv_gpio_set_output_data)
    drv_gpio_set_output_data                 0x00013409   Thumb Code    26  hal_gpio.o(i.drv_gpio_set_output_data)
    i.drv_lcdc_bcsa_config                   0x00013428   Section        0  drv_lcdc.o(i.drv_lcdc_bcsa_config)
    i.drv_lcdc_cfg_int_frame                 0x00013450   Section        0  drv_lcdc.o(i.drv_lcdc_cfg_int_frame)
    i.drv_lcdc_clear_int                     0x0001347c   Section        0  drv_lcdc.o(i.drv_lcdc_clear_int)
    drv_lcdc_clear_int                       0x0001347d   Thumb Code    20  drv_lcdc.o(i.drv_lcdc_clear_int)
    i.drv_lcdc_cmd_start                     0x00013494   Section        0  drv_lcdc.o(i.drv_lcdc_cmd_start)
    i.drv_lcdc_config_acc_command_mode       0x000134c8   Section        0  drv_lcdc.o(i.drv_lcdc_config_acc_command_mode)
    i.drv_lcdc_config_int                    0x000134dc   Section        0  drv_lcdc.o(i.drv_lcdc_config_int)
    i.drv_lcdc_config_int_single             0x00013514   Section        0  drv_lcdc.o(i.drv_lcdc_config_int_single)
    i.drv_lcdc_config_overwrite_rgb          0x0001353c   Section        0  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    i.drv_lcdc_config_src_parameter          0x00013554   Section        0  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    i.drv_lcdc_crop_hact                     0x000135a4   Section        0  drv_lcdc.o(i.drv_lcdc_crop_hact)
    i.drv_lcdc_ctrl_flow                     0x000135b4   Section        0  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    i.drv_lcdc_dith_config                   0x000135ec   Section        0  drv_lcdc.o(i.drv_lcdc_dith_config)
    i.drv_lcdc_edge_dect_config              0x0001361c   Section        0  drv_lcdc.o(i.drv_lcdc_edge_dect_config)
    i.drv_lcdc_edge_enh_config               0x00013658   Section        0  drv_lcdc.o(i.drv_lcdc_edge_enh_config)
    i.drv_lcdc_enable_shadow_reg             0x000136bc   Section        0  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    i.drv_lcdc_endianness_config             0x000136e0   Section        0  drv_lcdc.o(i.drv_lcdc_endianness_config)
    i.drv_lcdc_fc_config                     0x000136fc   Section        0  drv_lcdc.o(i.drv_lcdc_fc_config)
    i.drv_lcdc_fldc_config                   0x0001371c   Section        0  drv_lcdc.o(i.drv_lcdc_fldc_config)
    i.drv_lcdc_function_disable              0x00013740   Section        0  drv_lcdc.o(i.drv_lcdc_function_disable)
    i.drv_lcdc_function_enable               0x00013764   Section        0  drv_lcdc.o(i.drv_lcdc_function_enable)
    i.drv_lcdc_set_int                       0x00013788   Section        0  drv_lcdc.o(i.drv_lcdc_set_int)
    i.drv_lcdc_set_prefetch                  0x000137c4   Section        0  drv_lcdc.o(i.drv_lcdc_set_prefetch)
    i.drv_lcdc_set_tear_line                 0x000137e0   Section        0  drv_lcdc.o(i.drv_lcdc_set_tear_line)
    i.drv_lcdc_vid_hw_start                  0x000137fc   Section        0  drv_lcdc.o(i.drv_lcdc_vid_hw_start)
    i.drv_lcdc_vintp_mode_config             0x00013838   Section        0  drv_lcdc.o(i.drv_lcdc_vintp_mode_config)
    i.drv_memc_clear_status                  0x00013850   Section        0  drv_memc.o(i.drv_memc_clear_status)
    i.drv_memc_enable_irq                    0x00013864   Section        0  drv_memc.o(i.drv_memc_enable_irq)
    i.drv_memc_gen_a_tear_signal             0x000138a4   Section        0  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    i.drv_memc_get_status                    0x000138b4   Section        0  drv_memc.o(i.drv_memc_get_status)
    i.drv_memc_get_tear_mode                 0x000138cc   Section        0  drv_memc.o(i.drv_memc_get_tear_mode)
    i.drv_memc_rate_transfer_sel             0x000138dc   Section        0  drv_memc.o(i.drv_memc_rate_transfer_sel)
    i.drv_memc_sel_vsync                     0x000138f8   Section        0  drv_memc.o(i.drv_memc_sel_vsync)
    i.drv_memc_set_active_height             0x0001390c   Section        0  drv_memc.o(i.drv_memc_set_active_height)
    i.drv_memc_set_circ_mode_enable          0x00013924   Section        0  drv_memc.o(i.drv_memc_set_circ_mode_enable)
    i.drv_memc_set_data_mode                 0x00013940   Section        0  drv_memc.o(i.drv_memc_set_data_mode)
    i.drv_memc_set_double_buffer             0x00013954   Section        0  drv_memc.o(i.drv_memc_set_double_buffer)
    i.drv_memc_set_frame_drop_select         0x0001396c   Section        0  drv_memc.o(i.drv_memc_set_frame_drop_select)
    i.drv_memc_set_fs_en_conditions          0x00013988   Section        0  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    i.drv_memc_set_lcdc_st_conditions        0x000139a0   Section        0  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    i.drv_memc_set_ltpo_mode                 0x000139bc   Section        0  drv_memc.o(i.drv_memc_set_ltpo_mode)
    i.drv_memc_set_ltpo_pu_thres             0x000139dc   Section        0  drv_memc.o(i.drv_memc_set_ltpo_pu_thres)
    i.drv_memc_set_tear_mode                 0x000139f4   Section        0  drv_memc.o(i.drv_memc_set_tear_mode)
    i.drv_memc_set_tear_waveform             0x00013a08   Section        0  drv_memc.o(i.drv_memc_set_tear_waveform)
    i.drv_memc_set_vidc_sync_cnt             0x00013a34   Section        0  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    i.drv_phy_test_clear                     0x00013a48   Section        0  drv_phy_common.o(i.drv_phy_test_clear)
    i.drv_phy_test_lock                      0x00013a58   Section        0  drv_phy_common.o(i.drv_phy_test_lock)
    i.drv_pwr_efuse_pd                       0x00013a70   Section        0  drv_pwr.o(i.drv_pwr_efuse_pd)
    i.drv_pwr_get_power_ready_st             0x00013aa0   Section        0  drv_pwr.o(i.drv_pwr_get_power_ready_st)
    i.drv_pwr_set_digit_power_sel            0x00013ab0   Section        0  drv_pwr.o(i.drv_pwr_set_digit_power_sel)
    i.drv_pwr_set_pll_clk                    0x00013ad8   Section        0  drv_pwr.o(i.drv_pwr_set_pll_clk)
    i.drv_pwr_write_lock                     0x00013b0c   Section        0  drv_pwr.o(i.drv_pwr_write_lock)
    i.drv_rxbr_clear_pkt_buffer              0x00013b2c   Section        0  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    i.drv_rxbr_clear_status0                 0x00013b3c   Section        0  drv_rxbr.o(i.drv_rxbr_clear_status0)
    i.drv_rxbr_enable_irq                    0x00013b48   Section        0  drv_rxbr.o(i.drv_rxbr_enable_irq)
    i.drv_rxbr_frame_drop_cfg                0x00013ba4   Section        0  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    i.drv_rxbr_get_int_source                0x00013bc0   Section        0  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    drv_rxbr_get_int_source                  0x00013bc1   Thumb Code    20  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    i.drv_rxbr_get_status0                   0x00013bd8   Section        0  hal_internal_dcs.o(i.drv_rxbr_get_status0)
    drv_rxbr_get_status0                     0x00013bd9   Thumb Code    20  hal_internal_dcs.o(i.drv_rxbr_get_status0)
    i.drv_rxbr_hline_rcv1_cfg                0x00013bf0   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg)
    i.drv_rxbr_hline_rcv_cfg                 0x00013c04   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    i.drv_rxbr_register_irq1_callback        0x00013c14   Section        0  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    i.drv_rxbr_set_ack_pkt_header            0x00013c20   Section        0  drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header)
    i.drv_rxbr_set_color_format              0x00013c38   Section        0  drv_rxbr.o(i.drv_rxbr_set_color_format)
    i.drv_rxbr_set_filter_regs               0x00013c54   Section        0  drv_rxbr.o(i.drv_rxbr_set_filter_regs)
    i.drv_rxbr_set_inten                     0x00013c78   Section        0  drv_rxbr.o(i.drv_rxbr_set_inten)
    i.drv_rxbr_set_ltpo_drop_th              0x00013c94   Section        0  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    i.drv_rxbr_set_usr_cfg                   0x00013cac   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    i.drv_rxbr_set_usr_col                   0x00013cec   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    i.drv_rxbr_set_usr_row                   0x00013cfc   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    i.drv_se_init                            0x00013d0c   Section        0  drv_se.o(i.drv_se_init)
    i.drv_se_set_dsc                         0x00013d84   Section        0  drv_se.o(i.drv_se_set_dsc)
    i.drv_se_set_lcdc                        0x00013e58   Section        0  drv_se.o(i.drv_se_set_lcdc)
    i.drv_se_set_memc                        0x00013ee0   Section        0  drv_se.o(i.drv_se_set_memc)
    i.drv_se_set_rxbr                        0x00013f48   Section        0  drv_se.o(i.drv_se_set_rxbr)
    i.drv_se_set_vidc                        0x00014018   Section        0  drv_se.o(i.drv_se_set_vidc)
    i.drv_se_start_rx                        0x000140c4   Section        0  drv_se.o(i.drv_se_start_rx)
    i.drv_sys_cfg_clear_all_int              0x000140d8   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    i.drv_sys_cfg_clear_pending              0x000140e4   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    i.drv_sys_cfg_set_int                    0x0001410c   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    i.drv_timer_clear_status_flags           0x00014130   Section        0  drv_timer.o(i.drv_timer_clear_status_flags)
    drv_timer_clear_status_flags             0x00014131   Thumb Code    26  drv_timer.o(i.drv_timer_clear_status_flags)
    i.drv_timer_enable                       0x0001414a   Section        0  drv_timer.o(i.drv_timer_enable)
    i.drv_timer_get_instance                 0x0001416c   Section        0  drv_timer.o(i.drv_timer_get_instance)
    i.drv_timer_handle_interrupt             0x0001417c   Section        0  drv_timer.o(i.drv_timer_handle_interrupt)
    drv_timer_handle_interrupt               0x0001417d   Thumb Code    54  drv_timer.o(i.drv_timer_handle_interrupt)
    i.drv_timer_register_callback            0x000141b8   Section        0  drv_timer.o(i.drv_timer_register_callback)
    i.drv_timer_set_compare_val              0x000141cc   Section        0  drv_timer.o(i.drv_timer_set_compare_val)
    i.drv_timer_set_int                      0x0001420c   Section        0  drv_timer.o(i.drv_timer_set_int)
    i.drv_timer_set_prescaler                0x00014254   Section        0  drv_timer.o(i.drv_timer_set_prescaler)
    i.drv_timer_set_repeat                   0x0001427c   Section        0  drv_timer.o(i.drv_timer_set_repeat)
    i.drv_tx_phy_test_enter                  0x0001428c   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    i.drv_tx_phy_test_exit                   0x000142ac   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    i.drv_tx_phy_test_write_code             0x000142cc   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    i.drv_uart_abort_recv                    0x000142f4   Section        0  drv_uart.o(i.drv_uart_abort_recv)
    i.drv_uart_abort_send                    0x00014328   Section        0  drv_uart.o(i.drv_uart_abort_send)
    i.drv_uart_config_int                    0x0001435c   Section        0  drv_uart.o(i.drv_uart_config_int)
    i.drv_uart_enable_clk                    0x00014370   Section        0  drv_uart.o(i.drv_uart_enable_clk)
    drv_uart_enable_clk                      0x00014371   Thumb Code    24  drv_uart.o(i.drv_uart_enable_clk)
    i.drv_uart_enable_int                    0x00014388   Section        0  drv_uart.o(i.drv_uart_enable_int)
    i.drv_uart_get_instance                  0x000143e4   Section        0  drv_uart.o(i.drv_uart_get_instance)
    i.drv_uart_init                          0x0001440c   Section        0  drv_uart.o(i.drv_uart_init)
    i.drv_uart_int_trans_handle              0x000144dc   Section        0  drv_uart.o(i.drv_uart_int_trans_handle)
    drv_uart_int_trans_handle                0x000144dd   Thumb Code    54  drv_uart.o(i.drv_uart_int_trans_handle)
    i.drv_uart_reset_rx_fifo                 0x00014518   Section        0  drv_uart.o(i.drv_uart_reset_rx_fifo)
    i.drv_uart_reset_tx_fifo                 0x00014534   Section        0  drv_uart.o(i.drv_uart_reset_tx_fifo)
    i.drv_uart_send_blocking                 0x00014550   Section        0  drv_uart.o(i.drv_uart_send_blocking)
    i.drv_uart_set_baud_rate                 0x0001456a   Section        0  drv_uart.o(i.drv_uart_set_baud_rate)
    i.drv_uart_trans_create_handle           0x000145c0   Section        0  drv_uart.o(i.drv_uart_trans_create_handle)
    i.drv_vidc_clear_irq                     0x0001460c   Section        0  drv_vidc.o(i.drv_vidc_clear_irq)
    i.drv_vidc_enable                        0x0001461c   Section        0  drv_vidc.o(i.drv_vidc_enable)
    i.drv_vidc_enable_irq                    0x0001463c   Section        0  drv_vidc.o(i.drv_vidc_enable_irq)
    i.drv_vidc_get_int_source                0x0001467c   Section        0  drv_vidc.o(i.drv_vidc_get_int_source)
    i.drv_vidc_get_irq_status                0x000146a8   Section        0  drv_vidc.o(i.drv_vidc_get_irq_status)
    i.drv_vidc_init_module_enable            0x000146c0   Section        0  drv_vidc.o(i.drv_vidc_init_module_enable)
    i.drv_vidc_register_callback             0x000146ec   Section        0  drv_vidc.o(i.drv_vidc_register_callback)
    i.drv_vidc_reset                         0x000146f8   Section        0  drv_vidc.o(i.drv_vidc_reset)
    i.drv_vidc_set_circ_mode_enable          0x00014704   Section        0  drv_vidc.o(i.drv_vidc_set_circ_mode_enable)
    i.drv_vidc_set_dither_config             0x00014720   Section        0  drv_vidc.o(i.drv_vidc_set_dither_config)
    i.drv_vidc_set_dst_parameter             0x00014758   Section        0  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    i.drv_vidc_set_honly_hcoef0              0x000147b4   Section        0  drv_vidc.o(i.drv_vidc_set_honly_hcoef0)
    i.drv_vidc_set_honly_hinitb              0x000147c0   Section        0  drv_vidc.o(i.drv_vidc_set_honly_hinitb)
    i.drv_vidc_set_honly_hinitr              0x000147ec   Section        0  drv_vidc.o(i.drv_vidc_set_honly_hinitr)
    i.drv_vidc_set_irqen                     0x0001481c   Section        0  drv_vidc.o(i.drv_vidc_set_irqen)
    i.drv_vidc_set_mirror                    0x00014838   Section        0  drv_vidc.o(i.drv_vidc_set_mirror)
    i.drv_vidc_set_pentile_swap              0x0001484c   Section        0  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    i.drv_vidc_set_pu_ctrl                   0x00014868   Section        0  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    i.drv_vidc_set_rotation                  0x00014874   Section        0  drv_vidc.o(i.drv_vidc_set_rotation)
    i.drv_vidc_set_scld_hcoef0               0x0001488c   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    i.drv_vidc_set_scld_hcoef1               0x00014898   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    i.drv_vidc_set_scld_step                 0x000148a4   Section        0  drv_vidc.o(i.drv_vidc_set_scld_step)
    i.drv_vidc_set_scld_vcoef0               0x000148b8   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    i.drv_vidc_set_scld_vcoef1               0x000148c4   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    i.drv_vidc_set_src_parameter             0x000148d0   Section        0  drv_vidc.o(i.drv_vidc_set_src_parameter)
    i.drv_vidc_set_vintp_config              0x000148f0   Section        0  drv_vidc.o(i.drv_vidc_set_vintp_config)
    i.fputc                                  0x00014928   Section        0  tau_log.o(i.fputc)
    i.google_p6a_demo                        0x0001495c   Section        0  p6a_demo.o(i.google_p6a_demo)
    i.ha_intl_fb_check_pu_size               0x000149b8   Section        0  hal_internal_fb.o(i.ha_intl_fb_check_pu_size)
    ha_intl_fb_check_pu_size                 0x000149b9   Thumb Code    58  hal_internal_fb.o(i.ha_intl_fb_check_pu_size)
    i.hal_dsi_rx_ctrl_create_handle          0x000149f8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    i.hal_dsi_rx_ctrl_dcs_async_handler      0x00014a38   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler)
    i.hal_dsi_rx_ctrl_get_max_ret_size       0x00014a78   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size)
    i.hal_dsi_rx_ctrl_init                   0x00014a98   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    i.hal_dsi_rx_ctrl_init_clk               0x00014b44   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    hal_dsi_rx_ctrl_init_clk                 0x00014b45   Thumb Code   222  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    i.hal_dsi_rx_ctrl_init_dsi_rx            0x00014c44   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    hal_dsi_rx_ctrl_init_dsi_rx              0x00014c45   Thumb Code   232  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    i.hal_dsi_rx_ctrl_init_memc              0x00014d4c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    hal_dsi_rx_ctrl_init_memc                0x00014d4d   Thumb Code   294  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    i.hal_dsi_rx_ctrl_init_rxbr              0x00014e78   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    hal_dsi_rx_ctrl_init_rxbr                0x00014e79   Thumb Code   314  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    i.hal_dsi_rx_ctrl_init_vidc              0x00014fc0   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    hal_dsi_rx_ctrl_init_vidc                0x00014fc1   Thumb Code   624  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    i.hal_dsi_rx_ctrl_pre_init_pps           0x00015240   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    i.hal_dsi_rx_ctrl_send_ack_cmd           0x00015278   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd)
    i.hal_dsi_rx_ctrl_set_ipi_cfg            0x00015368   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    hal_dsi_rx_ctrl_set_ipi_cfg              0x00015369   Thumb Code    48  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    i.hal_dsi_rx_ctrl_start                  0x00015398   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    i.hal_dsi_rx_ctrl_toggle_resolution      0x000153c8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    i.hal_dsi_tx_cmd_mode_cal_timing         0x000153e8   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing)
    hal_dsi_tx_cmd_mode_cal_timing           0x000153e9   Thumb Code   510  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing)
    i.hal_dsi_tx_ctrl_create_handle          0x00015668   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    i.hal_dsi_tx_ctrl_gen_a_tear_signal      0x000156a0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal)
    i.hal_dsi_tx_ctrl_init                   0x000156c4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    i.hal_dsi_tx_ctrl_init_clk               0x00015740   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    hal_dsi_tx_ctrl_init_clk                 0x00015741   Thumb Code    12  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    i.hal_dsi_tx_ctrl_set_overwrite_rgb      0x00015750   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    i.hal_dsi_tx_ctrl_set_tear_mode          0x00015758   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode)
    i.hal_dsi_tx_ctrl_start                  0x00015764   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    i.hal_dsi_tx_ctrl_write_array_cmd        0x000157f4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd)
    i.hal_dsi_tx_ctrl_write_cmd              0x000158e8   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    i.hal_dsi_tx_init_cfg                    0x000159b8   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg)
    hal_dsi_tx_init_cfg                      0x000159b9   Thumb Code   250  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg)
    i.hal_dsi_tx_init_dpi_timing             0x00015abc   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing)
    hal_dsi_tx_init_dpi_timing               0x00015abd   Thumb Code    58  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing)
    i.hal_dsi_tx_init_phy_cfg                0x00015b00   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    hal_dsi_tx_init_phy_cfg                  0x00015b01   Thumb Code    22  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    i.hal_dsi_tx_init_timing                 0x00015b16   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing)
    hal_dsi_tx_init_timing                   0x00015b17   Thumb Code    82  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing)
    i.hal_dsi_tx_init_vid_timing             0x00015b68   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing)
    hal_dsi_tx_init_vid_timing               0x00015b69   Thumb Code    70  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing)
    i.hal_dsi_tx_send_cmd                    0x00015bbc   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    hal_dsi_tx_send_cmd                      0x00015bbd   Thumb Code    58  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    i.hal_dsi_tx_timing_info_update          0x00015bfc   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update)
    hal_dsi_tx_timing_info_update            0x00015bfd   Thumb Code   142  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update)
    i.hal_dsi_tx_vid_mode_cal_timing         0x00015c90   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing)
    hal_dsi_tx_vid_mode_cal_timing           0x00015c91   Thumb Code   766  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing)
    i.hal_gpio_config_pad                    0x00015fa0   Section        0  hal_gpio.o(i.hal_gpio_config_pad)
    i.hal_gpio_init_input                    0x00015fda   Section        0  hal_gpio.o(i.hal_gpio_init_input)
    i.hal_gpio_init_output                   0x00015ff0   Section        0  hal_gpio.o(i.hal_gpio_init_output)
    i.hal_gpio_set_mode                      0x0001600c   Section        0  hal_gpio.o(i.hal_gpio_set_mode)
    i.hal_gpio_set_output_data               0x0001606c   Section        0  hal_gpio.o(i.hal_gpio_set_output_data)
    i.hal_internal_sync_get_hight_performan_mode 0x00016074   Section        0  hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode)
    i.hal_internal_sync_input_resolution_change 0x00016084   Section        0  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    i.hal_internal_sync_register_lcdc_cb     0x00016238   Section        0  hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb)
    i.hal_internal_vsync_deinit              0x00016244   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    i.hal_internal_vsync_get_sync_line       0x00016264   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    i.hal_internal_vsync_get_tx_state        0x00016278   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    i.hal_internal_vsync_init_rx             0x00016284   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    i.hal_internal_vsync_init_tx             0x0001636c   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    i.hal_internal_vsync_set_rx_state        0x00016434   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    i.hal_internal_vsync_set_tear_mode       0x00016454   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    i.hal_internal_vsync_set_tx_state        0x00016640   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    i.hal_intl_dcs_init_sw_fltr              0x00016698   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr)
    i.hal_intl_dcs_rx_get_dcs_packet_data    0x00016704   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data)
    hal_intl_dcs_rx_get_dcs_packet_data      0x00016705   Thumb Code   782  hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data)
    i.hal_intl_dcs_rx_receive_packet         0x00016b34   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet)
    hal_intl_dcs_rx_receive_packet           0x00016b35   Thumb Code   122  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet)
    i.hal_intl_dcs_rx_receive_pps            0x00016bbc   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps)
    hal_intl_dcs_rx_receive_pps              0x00016bbd   Thumb Code   266  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps)
    i.hal_intl_dcs_set_auto_hw_filter        0x00016d30   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter)
    i.hal_intl_dcs_sw_filter_handle          0x00016dbc   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle)
    hal_intl_dcs_sw_filter_handle            0x00016dbd   Thumb Code    36  hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle)
    i.hal_intl_fb_cal_fb_info                0x00016de8   Section        0  hal_internal_fb.o(i.hal_intl_fb_cal_fb_info)
    i.hal_intl_fb_check_bandwidth            0x00017100   Section        0  hal_internal_fb.o(i.hal_intl_fb_check_bandwidth)
    hal_intl_fb_check_bandwidth              0x00017101   Thumb Code    92  hal_internal_fb.o(i.hal_intl_fb_check_bandwidth)
    i.hal_intl_fb_edge_resize                0x00017164   Section        0  hal_internal_fb.o(i.hal_intl_fb_edge_resize)
    hal_intl_fb_edge_resize                  0x00017165   Thumb Code   214  hal_internal_fb.o(i.hal_intl_fb_edge_resize)
    i.hal_intl_fb_flow_control_adapter       0x00017240   Section        0  hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter)
    hal_intl_fb_flow_control_adapter         0x00017241   Thumb Code   110  hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter)
    i.hal_intl_fb_get_memc_flow_mode         0x000172b4   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode)
    i.hal_intl_fb_get_rx_fb_info             0x000172c0   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info)
    i.hal_intl_fb_get_tx_fb_info             0x000172d0   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info)
    i.hal_intl_fb_get_user_flow              0x000172e0   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_user_flow)
    i.hal_intl_svs_deinit_rx                 0x000172ec   Section        0  hal_internal_svs.o(i.hal_intl_svs_deinit_rx)
    i.hal_intl_svs_deinit_tx                 0x00017314   Section        0  hal_internal_svs.o(i.hal_intl_svs_deinit_tx)
    i.hal_intl_svs_handle                    0x00017324   Section        0  hal_internal_svs.o(i.hal_intl_svs_handle)
    i.hal_intl_svs_init_rx                   0x00017348   Section        0  hal_internal_svs.o(i.hal_intl_svs_init_rx)
    i.hal_intl_svs_init_tx                   0x000173c8   Section        0  hal_internal_svs.o(i.hal_intl_svs_init_tx)
    i.hal_intl_svs_set_rx_vtt                0x000173dc   Section        0  hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt)
    i.hal_intl_svs_update_rxbr_clk           0x000173e8   Section        0  hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk)
    i.hal_lcdc_displayproc_config            0x00017430   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config)
    i.hal_lcdc_init_cfg                      0x000174a0   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    hal_lcdc_init_cfg                        0x000174a1   Thumb Code    62  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    i.hal_lcdc_init_clk                      0x000174de   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    hal_lcdc_init_clk                        0x000174df   Thumb Code   112  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    i.hal_lcdc_postproc_config               0x00017550   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config)
    i.hal_lcdc_start                         0x00017678   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_start)
    hal_lcdc_start                           0x00017679   Thumb Code    36  hal_dsi_tx_ctrl.o(i.hal_lcdc_start)
    i.hal_lcdc_timinggen_config              0x0001769c   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config)
    hal_lcdc_timinggen_config                0x0001769d   Thumb Code    60  hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config)
    i.hal_lcdc_upscaler_config               0x000176d8   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config)
    i.hal_nonshadow_func_update              0x000177b8   Section        0  hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update)
    i.hal_pwr_get_vcc_power_ready            0x00017874   Section        0  hal_pwr.o(i.hal_pwr_get_vcc_power_ready)
    i.hal_pwr_set_main_power                 0x0001787c   Section        0  hal_pwr.o(i.hal_pwr_set_main_power)
    i.hal_system_init                        0x00017884   Section        0  hal_system.o(i.hal_system_init)
    i.hal_system_updata_sysclk               0x00017968   Section        0  hal_system.o(i.hal_system_updata_sysclk)
    i.hal_timer_deinit                       0x000179b8   Section        0  hal_timer.o(i.hal_timer_deinit)
    i.hal_timer_init                         0x000179e8   Section        0  hal_timer.o(i.hal_timer_init)
    i.hal_timer_start                        0x00017a04   Section        0  hal_timer.o(i.hal_timer_start)
    i.hal_timer_stop                         0x00017a34   Section        0  hal_timer.o(i.hal_timer_stop)
    i.hal_tx_frame_rate_adjust               0x00017a5c   Section        0  hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust)
    hal_tx_frame_rate_adjust                 0x00017a5d   Thumb Code    44  hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust)
    i.hal_uart_init                          0x00017a8c   Section        0  hal_uart.o(i.hal_uart_init)
    i.hal_uart_send_blocking                 0x00017b20   Section        0  hal_uart.o(i.hal_uart_send_blocking)
    i.hal_vsync_func_update                  0x00017b3c   Section        0  hal_dsi_tx_ctrl.o(i.hal_vsync_func_update)
    i.hal_vsync_reset_lcdc_scaler            0x00017b54   Section        0  hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler)
    i.main                                   0x00017c34   Section        0  main.o(i.main)
    i.pps_update_handle                      0x00017c74   Section        0  p6a_demo.o(i.pps_update_handle)
    pps_update_handle                        0x00017c75   Thumb Code   104  p6a_demo.o(i.pps_update_handle)
    i.rxbr_irq1_callback                     0x00017ce4   Section        0  hal_internal_vsync.o(i.rxbr_irq1_callback)
    rxbr_irq1_callback                       0x00017ce5   Thumb Code   478  hal_internal_vsync.o(i.rxbr_irq1_callback)
    i.send_panel_init_code                   0x00017fc8   Section        0  p6a_demo.o(i.send_panel_init_code)
    send_panel_init_code                     0x00017fc9   Thumb Code    58  p6a_demo.o(i.send_panel_init_code)
    i.soft_double_buffer_update              0x00018004   Section        0  hal_internal_vsync.o(i.soft_double_buffer_update)
    soft_double_buffer_update                0x00018005   Thumb Code    56  hal_internal_vsync.o(i.soft_double_buffer_update)
    i.soft_gen_te                            0x00018048   Section        0  hal_internal_vsync.o(i.soft_gen_te)
    soft_gen_te                              0x00018049   Thumb Code    86  hal_internal_vsync.o(i.soft_gen_te)
    i.soft_gen_te_double_buffer              0x000180b4   Section        0  hal_internal_vsync.o(i.soft_gen_te_double_buffer)
    soft_gen_te_double_buffer                0x000180b5   Thumb Code   202  hal_internal_vsync.o(i.soft_gen_te_double_buffer)
    i.soft_pro_motion_init                   0x00018194   Section        0  hal_internal_vsync.o(i.soft_pro_motion_init)
    soft_pro_motion_init                     0x00018195   Thumb Code    46  hal_internal_vsync.o(i.soft_pro_motion_init)
    i.soft_swire_init                        0x000181cc   Section        0  p6a_demo.o(i.soft_swire_init)
    soft_swire_init                          0x000181cd   Thumb Code    48  p6a_demo.o(i.soft_swire_init)
    i.soft_swire_start                       0x00018204   Section        0  p6a_demo.o(i.soft_swire_start)
    soft_swire_start                         0x00018205   Thumb Code    46  p6a_demo.o(i.soft_swire_start)
    i.soft_swire_timer_callback              0x00018234   Section        0  p6a_demo.o(i.soft_swire_timer_callback)
    soft_swire_timer_callback                0x00018235   Thumb Code    64  p6a_demo.o(i.soft_swire_timer_callback)
    i.soft_tear_adjust_line                  0x0001827c   Section        0  hal_internal_vsync.o(i.soft_tear_adjust_line)
    soft_tear_adjust_line                    0x0001827d   Thumb Code    26  hal_internal_vsync.o(i.soft_tear_adjust_line)
    i.svs_direct_mode_setting                0x000182a0   Section        0  hal_internal_svs.o(i.svs_direct_mode_setting)
    svs_direct_mode_setting                  0x000182a1   Thumb Code   154  hal_internal_svs.o(i.svs_direct_mode_setting)
    i.svs_get_rel_intv                       0x0001834c   Section        0  hal_internal_svs.o(i.svs_get_rel_intv)
    svs_get_rel_intv                         0x0001834d   Thumb Code    20  hal_internal_svs.o(i.svs_get_rel_intv)
    i.svs_sync_handle                        0x00018368   Section        0  hal_internal_svs.o(i.svs_sync_handle)
    svs_sync_handle                          0x00018369   Thumb Code   158  hal_internal_svs.o(i.svs_sync_handle)
    i.svs_wait_fr_stab                       0x00018418   Section        0  hal_internal_svs.o(i.svs_wait_fr_stab)
    svs_wait_fr_stab                         0x00018419   Thumb Code   148  hal_internal_svs.o(i.svs_wait_fr_stab)
    i.svs_wait_start                         0x000184e4   Section        0  hal_internal_svs.o(i.svs_wait_start)
    svs_wait_start                           0x000184e5   Thumb Code   250  hal_internal_svs.o(i.svs_wait_start)
    i.tau_log_init                           0x000185f0   Section        0  tau_log.o(i.tau_log_init)
    i.tau_log_printf                         0x00018624   Section        0  tau_log.o(i.tau_log_printf)
    i.tau_log_push_log                       0x000186a8   Section        0  tau_log.o(i.tau_log_push_log)
    i.vidc_callback                          0x00018720   Section        0  hal_internal_vsync.o(i.vidc_callback)
    vidc_callback                            0x00018721   Thumb Code   150  hal_internal_vsync.o(i.vidc_callback)
    i.vpre_err_reset                         0x000187d4   Section        0  hal_internal_vsync.o(i.vpre_err_reset)
    vpre_err_reset                           0x000187d5   Thumb Code   254  hal_internal_vsync.o(i.vpre_err_reset)
    .constdata                               0x000188ec   Section     4268  p6a_demo.o(.constdata)
    g_cus_rx_dcs_execute_table               0x000188ec   Data          72  p6a_demo.o(.constdata)
    .constdata                               0x00019998   Section       40  hal_dsi_rx_ctrl.o(.constdata)
    .constdata                               0x000199c0   Section       28  hal_dsi_tx_ctrl.o(.constdata)
    .constdata                               0x000199dc   Section      182  hal_gpio.o(.constdata)
    s_gpio_map                               0x000199dc   Data         104  hal_gpio.o(.constdata)
    s_gpio_perf                              0x00019a44   Data          78  hal_gpio.o(.constdata)
    .constdata                               0x00019a94   Section       48  hal_uart.o(.constdata)
    .constdata                               0x00019ac4   Section       16  drv_uart.o(.constdata)
    .conststring                             0x00019ad4   Section       66  hal_dsi_rx_ctrl.o(.conststring)
    .conststring                             0x00019b18   Section      144  hal_internal_vsync.o(.conststring)
    .conststring                             0x00019ba8   Section       70  hal_internal_dcs.o(.conststring)
    .data                                    0x00070000   Section      161  p6a_demo.o(.data)
    g_rx_ctrl_handle                         0x00070000   Data           4  p6a_demo.o(.data)
    g_tx_ctrl_handle                         0x00070004   Data           4  p6a_demo.o(.data)
    panel_display_done                       0x00070008   Data           1  p6a_demo.o(.data)
    sg_system_resume                         0x00070009   Data           1  p6a_demo.o(.data)
    sg_system_suspend                        0x0007000a   Data           1  p6a_demo.o(.data)
    sg_exit_idle_mode_flag                   0x0007000b   Data           1  p6a_demo.o(.data)
    g_resolution_change                      0x0007000c   Data           1  p6a_demo.o(.data)
    pps_renew_flag                           0x00070010   Data           4  p6a_demo.o(.data)
    pwr_rst_flag                             0x00070014   Data           4  p6a_demo.o(.data)
    reg53_E8_fg                              0x000700a0   Data           1  p6a_demo.o(.data)
    .data                                    0x000700a4   Section       48  hal_dsi_rx_ctrl.o(.data)
    g_hw_auto_filter                         0x000700a4   Data           1  hal_dsi_rx_ctrl.o(.data)
    g_crc_check_enable                       0x000700a5   Data           1  hal_dsi_rx_ctrl.o(.data)
    g_esc_clk                                0x000700a8   Data           4  hal_dsi_rx_ctrl.o(.data)
    g_before_draw_col                        0x000700ac   Data           4  hal_dsi_rx_ctrl.o(.data)
    g_before_draw_page                       0x000700b0   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_step                                 0x000700b4   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_cmd_filter                           0x000700b8   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_x                                    0x000700bc   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_y                                    0x000700c0   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_value                                0x000700c4   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_x                                    0x000700c8   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_y                                    0x000700cc   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_value                                0x000700d0   Data           4  hal_dsi_rx_ctrl.o(.data)
    .data                                    0x000700d4   Section       92  hal_dsi_tx_ctrl.o(.data)
    sg_bta_vsync_flag                        0x000700d4   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_vsync_flag                            0x000700d5   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_enter_sleep_cmd                       0x000700d6   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_fldc_cg_mode                          0x000700d7   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_scl_fir                        0x000700d8   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_honly_bypass_fir                      0x000700d9   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_bcs                            0x000700da   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_enhc                           0x000700db   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_edge_dect                      0x000700dc   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_edge_enh                       0x000700dd   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_dith                           0x000700de   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_dith_judge                            0x000700df   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_endianness                            0x000700e0   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_test_pattern_en                       0x000700e1   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_dith_judge_thr                        0x000700e4   Data           4  hal_dsi_tx_ctrl.o(.data)
    sg_ccm_para                              0x000700e8   Data          36  hal_dsi_tx_ctrl.o(.data)
    sg_honly_para                            0x0007010c   Data          36  hal_dsi_tx_ctrl.o(.data)
    .data                                    0x00070130   Section        1  tau_log.o(.data)
    g_log_port                               0x00070130   Data           1  tau_log.o(.data)
    .data                                    0x00070134   Section       24  hal_uart.o(.data)
    sg_dma_callback                          0x00070144   Data           4  hal_uart.o(.data)
    sg_user_data                             0x00070148   Data           4  hal_uart.o(.data)
    .data                                    0x0007014c   Section       16  hal_internal_vsync.o(.data)
    s_te_refine_mode                         0x0007014c   Data           1  hal_internal_vsync.o(.data)
    .data                                    0x0007015c   Section       36  hal_internal_dcs.o(.data)
    g_imm_packet                             0x0007015c   Data          24  hal_internal_dcs.o(.data)
    g_cus_rx_write_cmd_handle                0x00070174   Data          12  hal_internal_dcs.o(.data)
    .data                                    0x00070180   Section       12  drv_common.o(.data)
    s_my_tick                                0x00070180   Data           4  drv_common.o(.data)
    .data                                    0x0007018c   Section        1  drv_common.o(.data)
    .data                                    0x00070190   Section        4  drv_gpio.o(.data)
    g_ap_reset_cb                            0x00070190   Data           4  drv_gpio.o(.data)
    .data                                    0x00070194   Section       80  drv_timer.o(.data)
    sg_timer_info                            0x00070194   Data          80  drv_timer.o(.data)
    .data                                    0x000701e4   Section        4  drv_se.o(.data)
    chip_info                                0x000701e4   Data           4  drv_se.o(.data)
    .data                                    0x000701e8   Section        1  drv_dsi_rx.o(.data)
    sg_rx_drv_level                          0x000701e8   Data           1  drv_dsi_rx.o(.data)
    .data                                    0x000701ec   Section        8  drv_rxbr.o(.data)
    .data                                    0x000701f4   Section        4  drv_vidc.o(.data)
    .data                                    0x000701f8   Section      400  drv_dma.o(.data)
    sg_dma_handle                            0x000701f8   Data         256  drv_dma.o(.data)
    .data                                    0x00070388   Section        4  stdout.o(.data)
    .bss                                     0x0007038c   Section      208  hal_dsi_rx_ctrl.o(.bss)
    g_rx_ctrl_handle                         0x0007038c   Data         208  hal_dsi_rx_ctrl.o(.bss)
    .bss                                     0x0007045c   Section      184  hal_dsi_tx_ctrl.o(.bss)
    g_tx_ctrl_handle                         0x0007045c   Data          92  hal_dsi_tx_ctrl.o(.bss)
    sg_dsi_tx_param                          0x000704b8   Data          92  hal_dsi_tx_ctrl.o(.bss)
    .bss                                     0x00070514   Section      256  tau_log.o(.bss)
    g_log_buf                                0x00070514   Data         256  tau_log.o(.bss)
    .bss                                     0x00070614   Section       68  hal_internal_vsync.o(.bss)
    .bss                                     0x00070658   Section     2048  hal_internal_dcs.o(.bss)
    .bss                                     0x00070e58   Section      255  hal_internal_dcs.o(.bss)
    g_imm_buffer                             0x00070e58   Data         255  hal_internal_dcs.o(.bss)
    .bss                                     0x00070f58   Section       68  hal_internal_fb.o(.bss)
    .bss                                     0x00070f9c   Section       68  hal_internal_svs.o(.bss)
    sg_sys_handler                           0x00070f9c   Data          68  hal_internal_svs.o(.bss)
    .bss                                     0x00070fe0   Section       64  drv_gpio.o(.bss)
    s_gpio_cb                                0x00070fe0   Data          64  drv_gpio.o(.bss)
    .bss                                     0x00071020   Section     4204  dcs_packet_fifo.o(.bss)
    .bss                                     0x0007208c   Section       16  drv_dma.o(.bss)
    sg_dma_int_list                          0x0007208c   Data          16  drv_dma.o(.bss)
    .bss                                     0x0007209c   Section       96  drv_uart.o(.bss)
    sg_uart_userdata                         0x0007209c   Data          96  drv_uart.o(.bss)
    STACK                                    0x00072100   Section     4096  startup_armcm0.o(STACK)

    Global Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    BuildAttributes$$THM_ISAv3M$S$PE$A:L22$X:L11$S22$IEEE1$IW$USESV6$~STKCKD$USESV7$~SHL$OTIME$ROPI$IEEEJ$EBA8$MICROLIB$REQ8$PRES8$EABIv2 0x00000000   Number         0  anon$$obj.o ABSOLUTE
    __ARM_use_no_argv                        0x00000000   Number         0  main.o ABSOLUTE
    _printf_a                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_c                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_charcount                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_d                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_e                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_f                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_flags                            0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_dec                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_hex                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_g                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_i                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_int_dec                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_l                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ll                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lld                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lli                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llo                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llu                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llx                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_dec                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_hex                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_oct                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ls                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_mbtowc                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_n                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_o                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_p                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_percent                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_pre_padding                      0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_return_value                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_s                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_sizespec                         0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_str                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_signed                  0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_unsigned                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_u                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wctomb                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_widthprec                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_x                                0x00000000   Number         0  stubs.o ABSOLUTE
    __cpp_initialize__aeabi_                  - Undefined Weak Reference
    __cxa_finalize                            - Undefined Weak Reference
    _clock_init                               - Undefined Weak Reference
    _microlib_exit                            - Undefined Weak Reference
    __Vectors_Size                           0x000000c0   Number         0  startup_armcm0.o ABSOLUTE
    __Vectors                                0x00010000   Data           4  startup_armcm0.o(RESET)
    __Vectors_End                            0x000100c0   Data           0  startup_armcm0.o(RESET)
    __main                                   0x000100c1   Thumb Code     0  entry.o(.ARM.Collect$$$$00000000)
    _main_stk                                0x000100c1   Thumb Code     0  entry2.o(.ARM.Collect$$$$00000001)
    _main_scatterload                        0x000100c5   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    __main_after_scatterload                 0x000100c9   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    _main_clock                              0x000100c9   Thumb Code     0  entry7b.o(.ARM.Collect$$$$00000008)
    _main_cpp_init                           0x000100c9   Thumb Code     0  entry8b.o(.ARM.Collect$$$$0000000A)
    _main_init                               0x000100c9   Thumb Code     0  entry9a.o(.ARM.Collect$$$$0000000B)
    __rt_final_cpp                           0x000100d1   Thumb Code     0  entry10a.o(.ARM.Collect$$$$0000000D)
    __rt_final_exit                          0x000100d1   Thumb Code     0  entry11a.o(.ARM.Collect$$$$0000000F)
    Reset_Handler                            0x000100d5   Thumb Code    28  startup_armcm0.o(.text)
    NMI_Handler                              0x000100f1   Thumb Code     2  startup_armcm0.o(.text)
    SVC_Handler                              0x000100f5   Thumb Code     2  startup_armcm0.o(.text)
    PendSV_Handler                           0x000100f7   Thumb Code     2  startup_armcm0.o(.text)
    FLSCTRL_IRQn_Handler                     0x00010107   Thumb Code     2  startup_armcm0.o(.text)
    WDG_IRQn_Handler                         0x00010113   Thumb Code     2  startup_armcm0.o(.text)
    I2C0_IRQn_Handler                        0x00010117   Thumb Code     2  startup_armcm0.o(.text)
    I2C1_IRQn_Handler                        0x00010119   Thumb Code     2  startup_armcm0.o(.text)
    SPIS_IRQn_Handler                        0x0001011b   Thumb Code     2  startup_armcm0.o(.text)
    SPIM_IRQn_Handler                        0x0001011d   Thumb Code     2  startup_armcm0.o(.text)
    I2C2_IRQn_Handler                        0x00010121   Thumb Code     2  startup_armcm0.o(.text)
    OTP_IRQn_Handler                         0x00010123   Thumb Code     2  startup_armcm0.o(.text)
    SWIRE_IRQn_Handler                       0x00010125   Thumb Code     2  startup_armcm0.o(.text)
    PVD_IRQn_Handler                         0x00010127   Thumb Code     2  startup_armcm0.o(.text)
    __aeabi_uidiv                            0x0001014d   Thumb Code     0  uidiv.o(.text)
    __aeabi_uidivmod                         0x0001014d   Thumb Code    44  uidiv.o(.text)
    __aeabi_idiv                             0x00010179   Thumb Code     0  idiv.o(.text)
    __aeabi_idivmod                          0x00010179   Thumb Code    40  idiv.o(.text)
    __aeabi_memcpy                           0x000101a1   Thumb Code    36  memcpya.o(.text)
    __aeabi_memcpy4                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memcpy8                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memset                           0x000101c5   Thumb Code    14  memseta.o(.text)
    __aeabi_memset4                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memset8                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr                           0x000101d3   Thumb Code     4  memseta.o(.text)
    __aeabi_memclr4                          0x000101d3   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr8                          0x000101d3   Thumb Code     0  memseta.o(.text)
    _memset$wrapper                          0x000101d7   Thumb Code    18  memseta.o(.text)
    strlen                                   0x000101e9   Thumb Code    14  strlen.o(.text)
    memcmp                                   0x000101f7   Thumb Code    26  memcmp.o(.text)
    __aeabi_fadd                             0x00010211   Thumb Code   162  fadd.o(.text)
    __aeabi_fsub                             0x000102b3   Thumb Code     8  fadd.o(.text)
    __aeabi_frsub                            0x000102bb   Thumb Code     8  fadd.o(.text)
    __aeabi_fmul                             0x000102c3   Thumb Code   122  fmul.o(.text)
    __aeabi_fdiv                             0x0001033d   Thumb Code   124  fdiv.o(.text)
    __ARM_scalbnf                            0x000103b9   Thumb Code    24  fscalb.o(.text)
    scalbnf                                  0x000103b9   Thumb Code     0  fscalb.o(.text)
    __aeabi_dadd                             0x000103d1   Thumb Code   328  dadd.o(.text)
    __aeabi_dsub                             0x00010519   Thumb Code    12  dadd.o(.text)
    __aeabi_drsub                            0x00010525   Thumb Code    12  dadd.o(.text)
    __aeabi_dmul                             0x00010535   Thumb Code   202  dmul.o(.text)
    __aeabi_ui2f                             0x00010605   Thumb Code    14  ffltui.o(.text)
    __aeabi_ui2d                             0x00010615   Thumb Code    24  dfltui.o(.text)
    __aeabi_f2uiz                            0x00010631   Thumb Code    40  ffixui.o(.text)
    __aeabi_d2uiz                            0x00010659   Thumb Code    50  dfixui.o(.text)
    __aeabi_f2d                              0x00010695   Thumb Code    40  f2d.o(.text)
    __aeabi_d2f                              0x000106bd   Thumb Code    56  d2f.o(.text)
    __aeabi_cfcmpeq                          0x000106f5   Thumb Code     0  cfcmple.o(.text)
    __aeabi_cfcmple                          0x000106f5   Thumb Code    20  cfcmple.o(.text)
    __aeabi_cfrcmple                         0x00010709   Thumb Code    20  cfrcmple.o(.text)
    __aeabi_uldivmod                         0x0001071d   Thumb Code    96  uldiv.o(.text)
    __aeabi_llsl                             0x0001077d   Thumb Code    32  llshl.o(.text)
    _ll_shift_l                              0x0001077d   Thumb Code     0  llshl.o(.text)
    __aeabi_llsr                             0x0001079d   Thumb Code    34  llushr.o(.text)
    _ll_ushift_r                             0x0001079d   Thumb Code     0  llushr.o(.text)
    __aeabi_lasr                             0x000107bf   Thumb Code    38  llsshr.o(.text)
    _ll_sshift_r                             0x000107bf   Thumb Code     0  llsshr.o(.text)
    __I$use$fp                               0x000107e5   Thumb Code     0  iusefp.o(.text)
    _float_round                             0x000107e5   Thumb Code    16  fepilogue.o(.text)
    _float_epilogue                          0x000107f5   Thumb Code   114  fepilogue.o(.text)
    _double_round                            0x00010867   Thumb Code    26  depilogue.o(.text)
    _double_epilogue                         0x00010881   Thumb Code   164  depilogue.o(.text)
    __aeabi_ddiv                             0x00010925   Thumb Code   234  ddiv.o(.text)
    __aeabi_d2ulz                            0x00010a15   Thumb Code    54  dfixul.o(.text)
    __aeabi_cdrcmple                         0x00010a55   Thumb Code    38  cdrcmple.o(.text)
    __scatterload                            0x00010a7d   Thumb Code    28  init.o(.text)
    __scatterload_rt2                        0x00010a7d   Thumb Code     0  init.o(.text)
    __decompress                             0x00010aa1   Thumb Code     0  __dczerorl2.o(.text)
    __decompress1                            0x00010aa1   Thumb Code    86  __dczerorl2.o(.text)
    AP_NRESET_IRQn_Handler                   0x00010af9   Thumb Code    22  drv_gpio.o(i.AP_NRESET_IRQn_Handler)
    DMA_IRQn_Handler                         0x00010b15   Thumb Code    78  drv_dma.o(i.DMA_IRQn_Handler)
    EXTI_INT0_IRQn_Handler                   0x00010b71   Thumb Code    10  drv_gpio.o(i.EXTI_INT0_IRQn_Handler)
    EXTI_INT1_IRQn_Handler                   0x00010b7b   Thumb Code    10  drv_gpio.o(i.EXTI_INT1_IRQn_Handler)
    EXTI_INT2_IRQn_Handler                   0x00010b85   Thumb Code    10  drv_gpio.o(i.EXTI_INT2_IRQn_Handler)
    EXTI_INT3_IRQn_Handler                   0x00010b8f   Thumb Code    10  drv_gpio.o(i.EXTI_INT3_IRQn_Handler)
    EXTI_INT4_IRQn_Handler                   0x00010b99   Thumb Code    10  drv_gpio.o(i.EXTI_INT4_IRQn_Handler)
    EXTI_INT5_IRQn_Handler                   0x00010ba3   Thumb Code    10  drv_gpio.o(i.EXTI_INT5_IRQn_Handler)
    EXTI_INT6_IRQn_Handler                   0x00010bad   Thumb Code    10  drv_gpio.o(i.EXTI_INT6_IRQn_Handler)
    EXTI_INT7_IRQn_Handler                   0x00010bb7   Thumb Code    10  drv_gpio.o(i.EXTI_INT7_IRQn_Handler)
    HardFault_Handler                        0x00010bc1   Thumb Code    14  drv_common.o(i.HardFault_Handler)
    LCDC_IRQn_Handler                        0x00010c09   Thumb Code   118  hal_internal_vsync.o(i.LCDC_IRQn_Handler)
    MEMC_IRQn_Handler                        0x00010d09   Thumb Code   154  drv_memc.o(i.MEMC_IRQn_Handler)
    MIPI_TX_IRQn_Handler                     0x00010da5   Thumb Code    70  drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler)
    SysTick_Handler                          0x00010e5d   Thumb Code    20  drv_common.o(i.SysTick_Handler)
    TIMER0_IRQn_Handler                      0x00010e75   Thumb Code    10  drv_timer.o(i.TIMER0_IRQn_Handler)
    TIMER1_IRQn_Handler                      0x00010e7f   Thumb Code    10  drv_timer.o(i.TIMER1_IRQn_Handler)
    TIMER2_IRQn_Handler                      0x00010e89   Thumb Code    10  drv_timer.o(i.TIMER2_IRQn_Handler)
    TIMER3_IRQn_Handler                      0x00010e93   Thumb Code    10  drv_timer.o(i.TIMER3_IRQn_Handler)
    VIDC_IRQn_Handler                        0x00010e9d   Thumb Code    22  drv_vidc.o(i.VIDC_IRQn_Handler)
    VPRE1_IRQn_Handler                       0x00010eb9   Thumb Code    22  drv_rxbr.o(i.VPRE1_IRQn_Handler)
    VPRE_IRQn_Handler                        0x00010ed5   Thumb Code   104  hal_internal_dcs.o(i.VPRE_IRQn_Handler)
    __0printf                                0x00010f41   Thumb Code    24  printfa.o(i.__0printf)
    __1printf                                0x00010f41   Thumb Code     0  printfa.o(i.__0printf)
    __2printf                                0x00010f41   Thumb Code     0  printfa.o(i.__0printf)
    __c89printf                              0x00010f41   Thumb Code     0  printfa.o(i.__0printf)
    printf                                   0x00010f41   Thumb Code     0  printfa.o(i.__0printf)
    __0vsprintf                              0x00010f61   Thumb Code    30  printfa.o(i.__0vsprintf)
    __1vsprintf                              0x00010f61   Thumb Code     0  printfa.o(i.__0vsprintf)
    __2vsprintf                              0x00010f61   Thumb Code     0  printfa.o(i.__0vsprintf)
    __c89vsprintf                            0x00010f61   Thumb Code     0  printfa.o(i.__0vsprintf)
    vsprintf                                 0x00010f61   Thumb Code     0  printfa.o(i.__0vsprintf)
    __ARM_clz                                0x00010f85   Thumb Code    46  depilogue.o(i.__ARM_clz)
    __ARM_common_switch8                     0x00010fb3   Thumb Code    26  hal_dsi_rx_ctrl.o(i.__ARM_common_switch8)
    __scatterload_copy                       0x00010fed   Thumb Code    14  handlers.o(i.__scatterload_copy)
    __scatterload_null                       0x00010ffb   Thumb Code     2  handlers.o(i.__scatterload_null)
    s_RAM_CK                                 0x00011000   Data          28  drv_common.o(.ARM.__at_0x11000)
    g_tau_log                                0x0001101c   Data          16  tau_log.o(.ARM.__at_0x1101C)
    sg_pq_para                               0x0001102c   Data          22  hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C)
    MIPI_RX_IRQn_Handler                     0x00011045   Thumb Code   354  drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler)
    UART_IRQn_Handler                        0x000113a9   Thumb Code   364  drv_uart.o(i.UART_IRQn_Handler)
    __scatterload_zeroinit                   0x00011541   Thumb Code    14  handlers.o(i.__scatterload_zeroinit)
    app_display_init                         0x0001211d   Thumb Code    30  p6a_demo.o(i.app_display_init)
    app_gpio_init                            0x0001213d   Thumb Code    22  p6a_demo.o(i.app_gpio_init)
    board_Init                               0x00012451   Thumb Code    20  board.o(i.board_Init)
    ceil                                     0x00012469   Thumb Code   180  ceil.o(i.ceil)
    dcs_packet_fifo_alloc                    0x000125e5   Thumb Code    80  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    dcs_packet_fifo_init                     0x0001263d   Thumb Code    18  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    dcs_packet_free_fifo_header              0x00012655   Thumb Code    60  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    dcs_packet_get_fifo_header               0x00012699   Thumb Code    26  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    delayMs                                  0x000126bd   Thumb Code    24  tau_delay.o(i.delayMs)
    delayUs                                  0x000126d5   Thumb Code    40  tau_delay.o(i.delayUs)
    drv_common_system_init                   0x00012701   Thumb Code     8  drv_common.o(i.drv_common_system_init)
    drv_crgu_enable_clock                    0x00012709   Thumb Code    54  drv_crgu.o(i.drv_crgu_enable_clock)
    drv_crgu_get_rxbr_clk                    0x00012745   Thumb Code    70  drv_crgu.o(i.drv_crgu_get_rxbr_clk)
    drv_crgu_set_ahb_clk                     0x000127ad   Thumb Code    34  drv_crgu.o(i.drv_crgu_set_ahb_clk)
    drv_crgu_set_dpi_clk                     0x000127d5   Thumb Code    54  drv_crgu.o(i.drv_crgu_set_dpi_clk)
    drv_crgu_set_dsc_clk                     0x00012811   Thumb Code    52  drv_crgu.o(i.drv_crgu_set_dsc_clk)
    drv_crgu_set_fb_clk                      0x00012849   Thumb Code    34  drv_crgu.o(i.drv_crgu_set_fb_clk)
    drv_crgu_set_lcdc_clk                    0x00012871   Thumb Code    36  drv_crgu.o(i.drv_crgu_set_lcdc_clk)
    drv_crgu_set_reset                       0x00012899   Thumb Code    20  drv_crgu.o(i.drv_crgu_set_reset)
    drv_crgu_set_rxbr_clk                    0x000128b1   Thumb Code    34  drv_crgu.o(i.drv_crgu_set_rxbr_clk)
    drv_crgu_set_vidc_clk                    0x000128d9   Thumb Code    36  drv_crgu.o(i.drv_crgu_set_vidc_clk)
    drv_dma_clear_status                     0x00012901   Thumb Code    20  drv_dma.o(i.drv_dma_clear_status)
    drv_dsc_dec_enable                       0x0001292d   Thumb Code    44  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    drv_dsc_dec_get_nslc                     0x00012965   Thumb Code    22  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    drv_dsc_dec_set_irqen                    0x00012985   Thumb Code    24  drv_dsc_dec.o(i.drv_dsc_dec_set_irqen)
    drv_dsi_rx_calc_ipi_tx_delay             0x000129a1   Thumb Code   252  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    drv_dsi_rx_enable_irq                    0x00012aad   Thumb Code    58  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    drv_dsi_rx_get_compression_en            0x00012b59   Thumb Code    10  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    drv_dsi_rx_get_ddi_crc_en                0x00012b69   Thumb Code    10  drv_dsi_rx.o(i.drv_dsi_rx_get_ddi_crc_en)
    drv_dsi_rx_get_max_ret_size              0x00012b79   Thumb Code     8  drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size)
    drv_dsi_rx_power_up                      0x00012b85   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    drv_dsi_rx_set_check_crc                 0x00012b9d   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc)
    drv_dsi_rx_set_ctrl_cfg                  0x00012bb9   Thumb Code    32  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    drv_dsi_rx_set_ddi_cfg                   0x00012bdd   Thumb Code    10  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    drv_dsi_rx_set_ddi_crc_en                0x00012bed   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_crc_en)
    drv_dsi_rx_set_inten                     0x00012c09   Thumb Code     8  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    drv_dsi_rx_set_ipi_cfg                   0x00012c15   Thumb Code    12  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    drv_dsi_rx_set_ipi_ycbcr_frmt            0x00012c25   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_ycbcr_frmt)
    drv_dsi_rx_set_lane_swap                 0x00012c41   Thumb Code    16  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    drv_dsi_rx_set_resp_cnt                  0x00012c55   Thumb Code    32  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    drv_dsi_rx_set_tear_resp_en              0x00012c79   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_tear_resp_en)
    drv_dsi_rx_set_up_phy                    0x00012c95   Thumb Code   224  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    drv_dsi_tx_command_header                0x00012d95   Thumb Code    18  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    drv_dsi_tx_command_mode_cfg              0x00012dad   Thumb Code    82  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    drv_dsi_tx_command_put_payload           0x00012e05   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    drv_dsi_tx_config_eotp                   0x00012e11   Thumb Code    26  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    drv_dsi_tx_config_int                    0x00012e31   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    drv_dsi_tx_dpi_lpcmd_time                0x00012e3d   Thumb Code    10  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    drv_dsi_tx_dpi_mode                      0x00012e4d   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    drv_dsi_tx_dpi_polarity                  0x00012e5d   Thumb Code    32  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    drv_dsi_tx_edpi_cmd_size                 0x00012e81   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    drv_dsi_tx_get_cmd_status                0x00012e8d   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    drv_dsi_tx_mode                          0x00012e99   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    drv_dsi_tx_phy_clock_lane_auto_lp        0x00012ea5   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    drv_dsi_tx_phy_clock_lane_req_hs         0x00012ec1   Thumb Code    26  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    drv_dsi_tx_phy_lane_mode                 0x00012ee1   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    drv_dsi_tx_phy_status_ready              0x00012ef1   Thumb Code   100  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    drv_dsi_tx_phy_status_stopstate          0x00012f59   Thumb Code    62  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    drv_dsi_tx_phy_test_setup                0x00012f9d   Thumb Code   314  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    drv_dsi_tx_phy_time_cfg                  0x000130ed   Thumb Code    28  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    drv_dsi_tx_powerup                       0x0001310d   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    drv_dsi_tx_response_mode                 0x00013119   Thumb Code    30  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    drv_dsi_tx_set_bta_ack                   0x0001313d   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    drv_dsi_tx_set_esc_div                   0x00013159   Thumb Code    14  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    drv_dsi_tx_set_int                       0x0001316d   Thumb Code    58  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    drv_dsi_tx_set_time_out_div              0x000131ad   Thumb Code    18  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    drv_dsi_tx_set_video_chunk               0x000131c5   Thumb Code    14  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    drv_dsi_tx_set_video_timing              0x000131d9   Thumb Code    30  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    drv_dsi_tx_shutdown                      0x000131fd   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    drv_dsi_tx_timeout_cfg                   0x00013209   Thumb Code    38  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    drv_dsi_tx_video_mode_cfg                0x00013235   Thumb Code   226  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    drv_efuse_enter_inactive                 0x0001331d   Thumb Code    54  drv_efuse.o(i.drv_efuse_enter_inactive)
    drv_efuse_int_enable                     0x00013353   Thumb Code    12  drv_efuse.o(i.drv_efuse_int_enable)
    drv_efuse_read                           0x0001335f   Thumb Code    58  drv_efuse.o(i.drv_efuse_read)
    drv_efuse_read_req                       0x00013399   Thumb Code    24  drv_efuse.o(i.drv_efuse_read_req)
    drv_gpio_set_ioe                         0x000133d5   Thumb Code    26  drv_gpio.o(i.drv_gpio_set_ioe)
    drv_gpio_set_mode                        0x000133f5   Thumb Code    16  drv_gpio.o(i.drv_gpio_set_mode)
    drv_lcdc_bcsa_config                     0x00013429   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_bcsa_config)
    drv_lcdc_cfg_int_frame                   0x00013451   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_cfg_int_frame)
    drv_lcdc_cmd_start                       0x00013495   Thumb Code    46  drv_lcdc.o(i.drv_lcdc_cmd_start)
    drv_lcdc_config_acc_command_mode         0x000134c9   Thumb Code    14  drv_lcdc.o(i.drv_lcdc_config_acc_command_mode)
    drv_lcdc_config_int                      0x000134dd   Thumb Code    50  drv_lcdc.o(i.drv_lcdc_config_int)
    drv_lcdc_config_int_single               0x00013515   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_int_single)
    drv_lcdc_config_overwrite_rgb            0x0001353d   Thumb Code    18  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    drv_lcdc_config_src_parameter            0x00013555   Thumb Code    72  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    drv_lcdc_crop_hact                       0x000135a5   Thumb Code    10  drv_lcdc.o(i.drv_lcdc_crop_hact)
    drv_lcdc_ctrl_flow                       0x000135b5   Thumb Code    50  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    drv_lcdc_dith_config                     0x000135ed   Thumb Code    40  drv_lcdc.o(i.drv_lcdc_dith_config)
    drv_lcdc_edge_dect_config                0x0001361d   Thumb Code    50  drv_lcdc.o(i.drv_lcdc_edge_dect_config)
    drv_lcdc_edge_enh_config                 0x00013659   Thumb Code    86  drv_lcdc.o(i.drv_lcdc_edge_enh_config)
    drv_lcdc_enable_shadow_reg               0x000136bd   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    drv_lcdc_endianness_config               0x000136e1   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_endianness_config)
    drv_lcdc_fc_config                       0x000136fd   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_fc_config)
    drv_lcdc_fldc_config                     0x0001371d   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_fldc_config)
    drv_lcdc_function_disable                0x00013741   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_function_disable)
    drv_lcdc_function_enable                 0x00013765   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_function_enable)
    drv_lcdc_set_int                         0x00013789   Thumb Code    54  drv_lcdc.o(i.drv_lcdc_set_int)
    drv_lcdc_set_prefetch                    0x000137c5   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_set_prefetch)
    drv_lcdc_set_tear_line                   0x000137e1   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_set_tear_line)
    drv_lcdc_vid_hw_start                    0x000137fd   Thumb Code    56  drv_lcdc.o(i.drv_lcdc_vid_hw_start)
    drv_lcdc_vintp_mode_config               0x00013839   Thumb Code    18  drv_lcdc.o(i.drv_lcdc_vintp_mode_config)
    drv_memc_clear_status                    0x00013851   Thumb Code    14  drv_memc.o(i.drv_memc_clear_status)
    drv_memc_enable_irq                      0x00013865   Thumb Code    58  drv_memc.o(i.drv_memc_enable_irq)
    drv_memc_gen_a_tear_signal               0x000138a5   Thumb Code    12  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    drv_memc_get_status                      0x000138b5   Thumb Code    20  drv_memc.o(i.drv_memc_get_status)
    drv_memc_get_tear_mode                   0x000138cd   Thumb Code    10  drv_memc.o(i.drv_memc_get_tear_mode)
    drv_memc_rate_transfer_sel               0x000138dd   Thumb Code    22  drv_memc.o(i.drv_memc_rate_transfer_sel)
    drv_memc_sel_vsync                       0x000138f9   Thumb Code    16  drv_memc.o(i.drv_memc_sel_vsync)
    drv_memc_set_active_height               0x0001390d   Thumb Code    16  drv_memc.o(i.drv_memc_set_active_height)
    drv_memc_set_circ_mode_enable            0x00013925   Thumb Code    24  drv_memc.o(i.drv_memc_set_circ_mode_enable)
    drv_memc_set_data_mode                   0x00013941   Thumb Code    14  drv_memc.o(i.drv_memc_set_data_mode)
    drv_memc_set_double_buffer               0x00013955   Thumb Code    18  drv_memc.o(i.drv_memc_set_double_buffer)
    drv_memc_set_frame_drop_select           0x0001396d   Thumb Code    24  drv_memc.o(i.drv_memc_set_frame_drop_select)
    drv_memc_set_fs_en_conditions            0x00013989   Thumb Code    18  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    drv_memc_set_lcdc_st_conditions          0x000139a1   Thumb Code    20  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    drv_memc_set_ltpo_mode                   0x000139bd   Thumb Code    28  drv_memc.o(i.drv_memc_set_ltpo_mode)
    drv_memc_set_ltpo_pu_thres               0x000139dd   Thumb Code    18  drv_memc.o(i.drv_memc_set_ltpo_pu_thres)
    drv_memc_set_tear_mode                   0x000139f5   Thumb Code    16  drv_memc.o(i.drv_memc_set_tear_mode)
    drv_memc_set_tear_waveform               0x00013a09   Thumb Code    36  drv_memc.o(i.drv_memc_set_tear_waveform)
    drv_memc_set_vidc_sync_cnt               0x00013a35   Thumb Code    16  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    drv_phy_test_clear                       0x00013a49   Thumb Code    16  drv_phy_common.o(i.drv_phy_test_clear)
    drv_phy_test_lock                        0x00013a59   Thumb Code    24  drv_phy_common.o(i.drv_phy_test_lock)
    drv_pwr_efuse_pd                         0x00013a71   Thumb Code    36  drv_pwr.o(i.drv_pwr_efuse_pd)
    drv_pwr_get_power_ready_st               0x00013aa1   Thumb Code    10  drv_pwr.o(i.drv_pwr_get_power_ready_st)
    drv_pwr_set_digit_power_sel              0x00013ab1   Thumb Code    34  drv_pwr.o(i.drv_pwr_set_digit_power_sel)
    drv_pwr_set_pll_clk                      0x00013ad9   Thumb Code    30  drv_pwr.o(i.drv_pwr_set_pll_clk)
    drv_pwr_write_lock                       0x00013b0d   Thumb Code    18  drv_pwr.o(i.drv_pwr_write_lock)
    drv_rxbr_clear_pkt_buffer                0x00013b2d   Thumb Code    12  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    drv_rxbr_clear_status0                   0x00013b3d   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_clear_status0)
    drv_rxbr_enable_irq                      0x00013b49   Thumb Code    90  drv_rxbr.o(i.drv_rxbr_enable_irq)
    drv_rxbr_frame_drop_cfg                  0x00013ba5   Thumb Code    18  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    drv_rxbr_hline_rcv1_cfg                  0x00013bf1   Thumb Code    14  drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg)
    drv_rxbr_hline_rcv_cfg                   0x00013c05   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    drv_rxbr_register_irq1_callback          0x00013c15   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    drv_rxbr_set_ack_pkt_header              0x00013c21   Thumb Code    18  drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header)
    drv_rxbr_set_color_format                0x00013c39   Thumb Code    24  drv_rxbr.o(i.drv_rxbr_set_color_format)
    drv_rxbr_set_filter_regs                 0x00013c55   Thumb Code    32  drv_rxbr.o(i.drv_rxbr_set_filter_regs)
    drv_rxbr_set_inten                       0x00013c79   Thumb Code    22  drv_rxbr.o(i.drv_rxbr_set_inten)
    drv_rxbr_set_ltpo_drop_th                0x00013c95   Thumb Code    18  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    drv_rxbr_set_usr_cfg                     0x00013cad   Thumb Code    56  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    drv_rxbr_set_usr_col                     0x00013ced   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    drv_rxbr_set_usr_row                     0x00013cfd   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    drv_se_init                              0x00013d0d   Thumb Code   106  drv_se.o(i.drv_se_init)
    drv_se_set_dsc                           0x00013d85   Thumb Code   162  drv_se.o(i.drv_se_set_dsc)
    drv_se_set_lcdc                          0x00013e59   Thumb Code    88  drv_se.o(i.drv_se_set_lcdc)
    drv_se_set_memc                          0x00013ee1   Thumb Code    54  drv_se.o(i.drv_se_set_memc)
    drv_se_set_rxbr                          0x00013f49   Thumb Code   158  drv_se.o(i.drv_se_set_rxbr)
    drv_se_set_vidc                          0x00014019   Thumb Code   122  drv_se.o(i.drv_se_set_vidc)
    drv_se_start_rx                          0x000140c5   Thumb Code    16  drv_se.o(i.drv_se_start_rx)
    drv_sys_cfg_clear_all_int                0x000140d9   Thumb Code     8  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    drv_sys_cfg_clear_pending                0x000140e5   Thumb Code    32  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    drv_sys_cfg_set_int                      0x0001410d   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    drv_timer_enable                         0x0001414b   Thumb Code    32  drv_timer.o(i.drv_timer_enable)
    drv_timer_get_instance                   0x0001416d   Thumb Code    10  drv_timer.o(i.drv_timer_get_instance)
    drv_timer_register_callback              0x000141b9   Thumb Code    14  drv_timer.o(i.drv_timer_register_callback)
    drv_timer_set_compare_val                0x000141cd   Thumb Code    50  drv_timer.o(i.drv_timer_set_compare_val)
    drv_timer_set_int                        0x0001420d   Thumb Code    68  drv_timer.o(i.drv_timer_set_int)
    drv_timer_set_prescaler                  0x00014255   Thumb Code    36  drv_timer.o(i.drv_timer_set_prescaler)
    drv_timer_set_repeat                     0x0001427d   Thumb Code    12  drv_timer.o(i.drv_timer_set_repeat)
    drv_tx_phy_test_enter                    0x0001428d   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    drv_tx_phy_test_exit                     0x000142ad   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    drv_tx_phy_test_write_code               0x000142cd   Thumb Code    34  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    drv_uart_abort_recv                      0x000142f5   Thumb Code    46  drv_uart.o(i.drv_uart_abort_recv)
    drv_uart_abort_send                      0x00014329   Thumb Code    46  drv_uart.o(i.drv_uart_abort_send)
    drv_uart_config_int                      0x0001435d   Thumb Code    20  drv_uart.o(i.drv_uart_config_int)
    drv_uart_enable_int                      0x00014389   Thumb Code    84  drv_uart.o(i.drv_uart_enable_int)
    drv_uart_get_instance                    0x000143e5   Thumb Code    36  drv_uart.o(i.drv_uart_get_instance)
    drv_uart_init                            0x0001440d   Thumb Code   206  drv_uart.o(i.drv_uart_init)
    drv_uart_reset_rx_fifo                   0x00014519   Thumb Code    28  drv_uart.o(i.drv_uart_reset_rx_fifo)
    drv_uart_reset_tx_fifo                   0x00014535   Thumb Code    28  drv_uart.o(i.drv_uart_reset_tx_fifo)
    drv_uart_send_blocking                   0x00014551   Thumb Code    26  drv_uart.o(i.drv_uart_send_blocking)
    drv_uart_set_baud_rate                   0x0001456b   Thumb Code    84  drv_uart.o(i.drv_uart_set_baud_rate)
    drv_uart_trans_create_handle             0x000145c1   Thumb Code    72  drv_uart.o(i.drv_uart_trans_create_handle)
    drv_vidc_clear_irq                       0x0001460d   Thumb Code    10  drv_vidc.o(i.drv_vidc_clear_irq)
    drv_vidc_enable                          0x0001461d   Thumb Code    26  drv_vidc.o(i.drv_vidc_enable)
    drv_vidc_enable_irq                      0x0001463d   Thumb Code    58  drv_vidc.o(i.drv_vidc_enable_irq)
    drv_vidc_get_int_source                  0x0001467d   Thumb Code    40  drv_vidc.o(i.drv_vidc_get_int_source)
    drv_vidc_get_irq_status                  0x000146a9   Thumb Code    20  drv_vidc.o(i.drv_vidc_get_irq_status)
    drv_vidc_init_module_enable              0x000146c1   Thumb Code    36  drv_vidc.o(i.drv_vidc_init_module_enable)
    drv_vidc_register_callback               0x000146ed   Thumb Code     6  drv_vidc.o(i.drv_vidc_register_callback)
    drv_vidc_reset                           0x000146f9   Thumb Code     8  drv_vidc.o(i.drv_vidc_reset)
    drv_vidc_set_circ_mode_enable            0x00014705   Thumb Code    24  drv_vidc.o(i.drv_vidc_set_circ_mode_enable)
    drv_vidc_set_dither_config               0x00014721   Thumb Code    50  drv_vidc.o(i.drv_vidc_set_dither_config)
    drv_vidc_set_dst_parameter               0x00014759   Thumb Code    86  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    drv_vidc_set_honly_hcoef0                0x000147b5   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_honly_hcoef0)
    drv_vidc_set_honly_hinitb                0x000147c1   Thumb Code    38  drv_vidc.o(i.drv_vidc_set_honly_hinitb)
    drv_vidc_set_honly_hinitr                0x000147ed   Thumb Code    42  drv_vidc.o(i.drv_vidc_set_honly_hinitr)
    drv_vidc_set_irqen                       0x0001481d   Thumb Code    22  drv_vidc.o(i.drv_vidc_set_irqen)
    drv_vidc_set_mirror                      0x00014839   Thumb Code    16  drv_vidc.o(i.drv_vidc_set_mirror)
    drv_vidc_set_pentile_swap                0x0001484d   Thumb Code    20  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    drv_vidc_set_pu_ctrl                     0x00014869   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    drv_vidc_set_rotation                    0x00014875   Thumb Code    18  drv_vidc.o(i.drv_vidc_set_rotation)
    drv_vidc_set_scld_hcoef0                 0x0001488d   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    drv_vidc_set_scld_hcoef1                 0x00014899   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    drv_vidc_set_scld_step                   0x000148a5   Thumb Code    14  drv_vidc.o(i.drv_vidc_set_scld_step)
    drv_vidc_set_scld_vcoef0                 0x000148b9   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    drv_vidc_set_scld_vcoef1                 0x000148c5   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    drv_vidc_set_src_parameter               0x000148d1   Thumb Code    28  drv_vidc.o(i.drv_vidc_set_src_parameter)
    drv_vidc_set_vintp_config                0x000148f1   Thumb Code    52  drv_vidc.o(i.drv_vidc_set_vintp_config)
    fputc                                    0x00014929   Thumb Code    42  tau_log.o(i.fputc)
    google_p6a_demo                          0x0001495d   Thumb Code    44  p6a_demo.o(i.google_p6a_demo)
    hal_dsi_rx_ctrl_create_handle            0x000149f9   Thumb Code    60  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    hal_dsi_rx_ctrl_dcs_async_handler        0x00014a39   Thumb Code    60  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler)
    hal_dsi_rx_ctrl_get_max_ret_size         0x00014a79   Thumb Code    28  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size)
    hal_dsi_rx_ctrl_init                     0x00014a99   Thumb Code   158  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    hal_dsi_rx_ctrl_pre_init_pps             0x00015241   Thumb Code    50  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    hal_dsi_rx_ctrl_send_ack_cmd             0x00015279   Thumb Code   210  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd)
    hal_dsi_rx_ctrl_start                    0x00015399   Thumb Code    42  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    hal_dsi_rx_ctrl_toggle_resolution        0x000153c9   Thumb Code    28  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    hal_dsi_tx_ctrl_create_handle            0x00015669   Thumb Code    48  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    hal_dsi_tx_ctrl_gen_a_tear_signal        0x000156a1   Thumb Code    34  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal)
    hal_dsi_tx_ctrl_init                     0x000156c5   Thumb Code   110  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    hal_dsi_tx_ctrl_set_overwrite_rgb        0x00015751   Thumb Code     8  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    hal_dsi_tx_ctrl_set_tear_mode            0x00015759   Thumb Code    10  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode)
    hal_dsi_tx_ctrl_start                    0x00015765   Thumb Code   134  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    hal_dsi_tx_ctrl_write_array_cmd          0x000157f5   Thumb Code   238  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd)
    hal_dsi_tx_ctrl_write_cmd                0x000158e9   Thumb Code   202  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    hal_gpio_config_pad                      0x00015fa1   Thumb Code    58  hal_gpio.o(i.hal_gpio_config_pad)
    hal_gpio_init_input                      0x00015fdb   Thumb Code    22  hal_gpio.o(i.hal_gpio_init_input)
    hal_gpio_init_output                     0x00015ff1   Thumb Code    28  hal_gpio.o(i.hal_gpio_init_output)
    hal_gpio_set_mode                        0x0001600d   Thumb Code    92  hal_gpio.o(i.hal_gpio_set_mode)
    hal_gpio_set_output_data                 0x0001606d   Thumb Code     8  hal_gpio.o(i.hal_gpio_set_output_data)
    hal_internal_sync_get_hight_performan_mode 0x00016075   Thumb Code    10  hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode)
    hal_internal_sync_input_resolution_change 0x00016085   Thumb Code   336  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    hal_internal_sync_register_lcdc_cb       0x00016239   Thumb Code     8  hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb)
    hal_internal_vsync_deinit                0x00016245   Thumb Code    22  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    hal_internal_vsync_get_sync_line         0x00016265   Thumb Code    16  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    hal_internal_vsync_get_tx_state          0x00016279   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    hal_internal_vsync_init_rx               0x00016285   Thumb Code   206  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    hal_internal_vsync_init_tx               0x0001636d   Thumb Code   194  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    hal_internal_vsync_set_rx_state          0x00016435   Thumb Code    28  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    hal_internal_vsync_set_tear_mode         0x00016455   Thumb Code   424  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    hal_internal_vsync_set_tx_state          0x00016641   Thumb Code    78  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    hal_intl_dcs_init_sw_fltr                0x00016699   Thumb Code    90  hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr)
    hal_intl_dcs_set_auto_hw_filter          0x00016d31   Thumb Code   130  hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter)
    hal_intl_fb_cal_fb_info                  0x00016de9   Thumb Code   780  hal_internal_fb.o(i.hal_intl_fb_cal_fb_info)
    hal_intl_fb_get_memc_flow_mode           0x000172b5   Thumb Code     6  hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode)
    hal_intl_fb_get_rx_fb_info               0x000172c1   Thumb Code    12  hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info)
    hal_intl_fb_get_tx_fb_info               0x000172d1   Thumb Code    12  hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info)
    hal_intl_fb_get_user_flow                0x000172e1   Thumb Code     6  hal_internal_fb.o(i.hal_intl_fb_get_user_flow)
    hal_intl_svs_deinit_rx                   0x000172ed   Thumb Code    32  hal_internal_svs.o(i.hal_intl_svs_deinit_rx)
    hal_intl_svs_deinit_tx                   0x00017315   Thumb Code    10  hal_internal_svs.o(i.hal_intl_svs_deinit_tx)
    hal_intl_svs_handle                      0x00017325   Thumb Code    24  hal_internal_svs.o(i.hal_intl_svs_handle)
    hal_intl_svs_init_rx                     0x00017349   Thumb Code   120  hal_internal_svs.o(i.hal_intl_svs_init_rx)
    hal_intl_svs_init_tx                     0x000173c9   Thumb Code    16  hal_internal_svs.o(i.hal_intl_svs_init_tx)
    hal_intl_svs_set_rx_vtt                  0x000173dd   Thumb Code     6  hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt)
    hal_intl_svs_update_rxbr_clk             0x000173e9   Thumb Code    52  hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk)
    hal_lcdc_displayproc_config              0x00017431   Thumb Code    94  hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config)
    hal_lcdc_postproc_config                 0x00017551   Thumb Code   276  hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config)
    hal_lcdc_upscaler_config                 0x000176d9   Thumb Code   202  hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config)
    hal_nonshadow_func_update                0x000177b9   Thumb Code   180  hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update)
    hal_pwr_get_vcc_power_ready              0x00017875   Thumb Code     8  hal_pwr.o(i.hal_pwr_get_vcc_power_ready)
    hal_pwr_set_main_power                   0x0001787d   Thumb Code     8  hal_pwr.o(i.hal_pwr_set_main_power)
    hal_system_init                          0x00017885   Thumb Code   192  hal_system.o(i.hal_system_init)
    hal_system_updata_sysclk                 0x00017969   Thumb Code    60  hal_system.o(i.hal_system_updata_sysclk)
    hal_timer_deinit                         0x000179b9   Thumb Code    48  hal_timer.o(i.hal_timer_deinit)
    hal_timer_init                           0x000179e9   Thumb Code    28  hal_timer.o(i.hal_timer_init)
    hal_timer_start                          0x00017a05   Thumb Code    48  hal_timer.o(i.hal_timer_start)
    hal_timer_stop                           0x00017a35   Thumb Code    40  hal_timer.o(i.hal_timer_stop)
    hal_uart_init                            0x00017a8d   Thumb Code   134  hal_uart.o(i.hal_uart_init)
    hal_uart_send_blocking                   0x00017b21   Thumb Code    24  hal_uart.o(i.hal_uart_send_blocking)
    hal_vsync_func_update                    0x00017b3d   Thumb Code    18  hal_dsi_tx_ctrl.o(i.hal_vsync_func_update)
    hal_vsync_reset_lcdc_scaler              0x00017b55   Thumb Code   206  hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler)
    main                                     0x00017c35   Thumb Code    32  main.o(i.main)
    tau_log_init                             0x000185f1   Thumb Code    48  tau_log.o(i.tau_log_init)
    tau_log_printf                           0x00018625   Thumb Code   116  tau_log.o(i.tau_log_printf)
    tau_log_push_log                         0x000186a9   Thumb Code   118  tau_log.o(i.tau_log_push_log)
    panel_init_code                          0x00018934   Data        4177  p6a_demo.o(.constdata)
    Region$$Table$$Base                      0x00019bf0   Number         0  anon$$obj.o(Region$$Table)
    Region$$Table$$Limit                     0x00019c10   Number         0  anon$$obj.o(Region$$Table)
    s_swire_pwm_counter                      0x00070018   Data           1  p6a_demo.o(.data)
    rd_51_val                                0x0007001a   Data           2  p6a_demo.o(.data)
    rd_51_val2                               0x0007001c   Data           2  p6a_demo.o(.data)
    pps                                      0x0007001e   Data         128  p6a_demo.o(.data)
    value_51H                                0x0007009e   Data           1  p6a_demo.o(.data)
    value_51L                                0x0007009f   Data           1  p6a_demo.o(.data)
    sg_uart0_tx_handle                       0x00070134   Data           4  hal_uart.o(.data)
    sg_uart0_rx_handle                       0x00070138   Data           4  hal_uart.o(.data)
    sg_uart1_tx_handle                       0x0007013c   Data           4  hal_uart.o(.data)
    sg_uart1_rx_handle                       0x00070140   Data           4  hal_uart.o(.data)
    g_sof_gen_te_func                        0x00070150   Data           4  hal_internal_vsync.o(.data)
    hal_internal_vsync_handle_callback       0x00070154   Data           4  hal_internal_vsync.o(.data)
    hal_internal_disp_end_handle_callback    0x00070158   Data           4  hal_internal_vsync.o(.data)
    g_systick_cb_func                        0x00070184   Data           4  drv_common.o(.data)
    g_system_clock                           0x00070188   Data           4  drv_common.o(.data)
    g_system_delay_step                      0x0007018c   Data           1  drv_common.o(.data)
    g_int_rxbr_irq0_cb_func                  0x000701ec   Data           4  drv_rxbr.o(.data)
    g_int_rxbr_irq1_cb_func                  0x000701f0   Data           4  drv_rxbr.o(.data)
    g_int_vidc_cb_func                       0x000701f4   Data           4  drv_vidc.o(.data)
    dma_req_map                              0x000702f8   Data         144  drv_dma.o(.data)
    __stdout                                 0x00070388   Data           4  stdout.o(.data)
    g_vsync_handle                           0x00070614   Data          40  hal_internal_vsync.o(.bss)
    sg_pro_motion_handle                     0x0007063c   Data          28  hal_internal_vsync.o(.bss)
    g_dcs_execute_table                      0x00070658   Data        2048  hal_internal_dcs.o(.bss)
    g_rx_fb_info                             0x00070f58   Data          68  hal_internal_fb.o(.bss)
    g_packet_fifo                            0x00071020   Data        4204  dcs_packet_fifo.o(.bss)
    __stack_limit                            0x00072100   Data           0  startup_armcm0.o(STACK)
    __initial_sp                             0x00073100   Data           0  startup_armcm0.o(STACK)



==============================================================================

Memory Map of the image

  Image Entry point : 0x000100c1

  Load Region LR_IROM2 (Base: 0x00010000, Size: 0x00009f9c, Max: 0x00010000, ABSOLUTE, COMPRESSED[0x00009d5c])

    Execution Region ER_IROM2 (Exec base: 0x00010000, Load base: 0x00010000, Size: 0x00009c10, Max: 0x00010000, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00010000   0x00010000   0x000000c0   Data   RO          333    RESET               startup_armcm0.o
    0x000100c0   0x000100c0   0x00000000   Code   RO         1848  * .ARM.Collect$$$$00000000  mc_p.l(entry.o)
    0x000100c0   0x000100c0   0x00000004   Code   RO         2156    .ARM.Collect$$$$00000001  mc_p.l(entry2.o)
    0x000100c4   0x000100c4   0x00000004   Code   RO         2159    .ARM.Collect$$$$00000004  mc_p.l(entry5.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         2161    .ARM.Collect$$$$00000008  mc_p.l(entry7b.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         2163    .ARM.Collect$$$$0000000A  mc_p.l(entry8b.o)
    0x000100c8   0x000100c8   0x00000008   Code   RO         2164    .ARM.Collect$$$$0000000B  mc_p.l(entry9a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         2166    .ARM.Collect$$$$0000000D  mc_p.l(entry10a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         2168    .ARM.Collect$$$$0000000F  mc_p.l(entry11a.o)
    0x000100d0   0x000100d0   0x00000004   Code   RO         2157    .ARM.Collect$$$$00002712  mc_p.l(entry2.o)
    0x000100d4   0x000100d4   0x00000078   Code   RO          334    .text               startup_armcm0.o
    0x0001014c   0x0001014c   0x0000002c   Code   RO         1851    .text               mc_p.l(uidiv.o)
    0x00010178   0x00010178   0x00000028   Code   RO         1853    .text               mc_p.l(idiv.o)
    0x000101a0   0x000101a0   0x00000024   Code   RO         1855    .text               mc_p.l(memcpya.o)
    0x000101c4   0x000101c4   0x00000024   Code   RO         1857    .text               mc_p.l(memseta.o)
    0x000101e8   0x000101e8   0x0000000e   Code   RO         1859    .text               mc_p.l(strlen.o)
    0x000101f6   0x000101f6   0x0000001a   Code   RO         1861    .text               mc_p.l(memcmp.o)
    0x00010210   0x00010210   0x000000b2   Code   RO         2126    .text               mf_p.l(fadd.o)
    0x000102c2   0x000102c2   0x0000007a   Code   RO         2128    .text               mf_p.l(fmul.o)
    0x0001033c   0x0001033c   0x0000007c   Code   RO         2130    .text               mf_p.l(fdiv.o)
    0x000103b8   0x000103b8   0x00000018   Code   RO         2132    .text               mf_p.l(fscalb.o)
    0x000103d0   0x000103d0   0x00000164   Code   RO         2134    .text               mf_p.l(dadd.o)
    0x00010534   0x00010534   0x000000d0   Code   RO         2136    .text               mf_p.l(dmul.o)
    0x00010604   0x00010604   0x0000000e   Code   RO         2140    .text               mf_p.l(ffltui.o)
    0x00010612   0x00010612   0x00000002   PAD
    0x00010614   0x00010614   0x0000001c   Code   RO         2142    .text               mf_p.l(dfltui.o)
    0x00010630   0x00010630   0x00000028   Code   RO         2144    .text               mf_p.l(ffixui.o)
    0x00010658   0x00010658   0x0000003c   Code   RO         2146    .text               mf_p.l(dfixui.o)
    0x00010694   0x00010694   0x00000028   Code   RO         2148    .text               mf_p.l(f2d.o)
    0x000106bc   0x000106bc   0x00000038   Code   RO         2150    .text               mf_p.l(d2f.o)
    0x000106f4   0x000106f4   0x00000014   Code   RO         2152    .text               mf_p.l(cfcmple.o)
    0x00010708   0x00010708   0x00000014   Code   RO         2154    .text               mf_p.l(cfrcmple.o)
    0x0001071c   0x0001071c   0x00000060   Code   RO         2171    .text               mc_p.l(uldiv.o)
    0x0001077c   0x0001077c   0x00000020   Code   RO         2173    .text               mc_p.l(llshl.o)
    0x0001079c   0x0001079c   0x00000022   Code   RO         2175    .text               mc_p.l(llushr.o)
    0x000107be   0x000107be   0x00000026   Code   RO         2177    .text               mc_p.l(llsshr.o)
    0x000107e4   0x000107e4   0x00000000   Code   RO         2179    .text               mc_p.l(iusefp.o)
    0x000107e4   0x000107e4   0x00000082   Code   RO         2180    .text               mf_p.l(fepilogue.o)
    0x00010866   0x00010866   0x000000be   Code   RO         2182    .text               mf_p.l(depilogue.o)
    0x00010924   0x00010924   0x000000f0   Code   RO         2186    .text               mf_p.l(ddiv.o)
    0x00010a14   0x00010a14   0x00000040   Code   RO         2188    .text               mf_p.l(dfixul.o)
    0x00010a54   0x00010a54   0x00000028   Code   RO         2190    .text               mf_p.l(cdrcmple.o)
    0x00010a7c   0x00010a7c   0x00000024   Code   RO         2192    .text               mc_p.l(init.o)
    0x00010aa0   0x00010aa0   0x00000056   Code   RO         2202    .text               mc_p.l(__dczerorl2.o)
    0x00010af6   0x00010af6   0x00000002   PAD
    0x00010af8   0x00010af8   0x0000001c   Code   RO          953    i.AP_NRESET_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010b14   0x00010b14   0x0000005c   Code   RO         1697    i.DMA_IRQn_Handler  CVWL668T.lib(drv_dma.o)
    0x00010b70   0x00010b70   0x0000000a   Code   RO          954    i.EXTI_INT0_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010b7a   0x00010b7a   0x0000000a   Code   RO          955    i.EXTI_INT1_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010b84   0x00010b84   0x0000000a   Code   RO          956    i.EXTI_INT2_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010b8e   0x00010b8e   0x0000000a   Code   RO          957    i.EXTI_INT3_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010b98   0x00010b98   0x0000000a   Code   RO          958    i.EXTI_INT4_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010ba2   0x00010ba2   0x0000000a   Code   RO          959    i.EXTI_INT5_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010bac   0x00010bac   0x0000000a   Code   RO          960    i.EXTI_INT6_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010bb6   0x00010bb6   0x0000000a   Code   RO          961    i.EXTI_INT7_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010bc0   0x00010bc0   0x00000048   Code   RO          876    i.HardFault_Handler  CVWL668T.lib(drv_common.o)
    0x00010c08   0x00010c08   0x00000100   Code   RO          721    i.LCDC_IRQn_Handler  CVWL668T.lib(hal_internal_vsync.o)
    0x00010d08   0x00010d08   0x0000009a   Code   RO         1457    i.MEMC_IRQn_Handler  CVWL668T.lib(drv_memc.o)
    0x00010da2   0x00010da2   0x00000002   PAD
    0x00010da4   0x00010da4   0x000000b8   Code   RO         1263    i.MIPI_TX_IRQn_Handler  CVWL668T.lib(drv_dsi_tx.o)
    0x00010e5c   0x00010e5c   0x00000018   Code   RO          877    i.SysTick_Handler   CVWL668T.lib(drv_common.o)
    0x00010e74   0x00010e74   0x0000000a   Code   RO         1135    i.TIMER0_IRQn_Handler  CVWL668T.lib(drv_timer.o)
    0x00010e7e   0x00010e7e   0x0000000a   Code   RO         1136    i.TIMER1_IRQn_Handler  CVWL668T.lib(drv_timer.o)
    0x00010e88   0x00010e88   0x0000000a   Code   RO         1137    i.TIMER2_IRQn_Handler  CVWL668T.lib(drv_timer.o)
    0x00010e92   0x00010e92   0x0000000a   Code   RO         1138    i.TIMER3_IRQn_Handler  CVWL668T.lib(drv_timer.o)
    0x00010e9c   0x00010e9c   0x0000001c   Code   RO         1612    i.VIDC_IRQn_Handler  CVWL668T.lib(drv_vidc.o)
    0x00010eb8   0x00010eb8   0x0000001c   Code   RO         1523    i.VPRE1_IRQn_Handler  CVWL668T.lib(drv_rxbr.o)
    0x00010ed4   0x00010ed4   0x0000006c   Code   RO          787    i.VPRE_IRQn_Handler  CVWL668T.lib(hal_internal_dcs.o)
    0x00010f40   0x00010f40   0x00000020   Code   RO         2098    i.__0printf         mc_p.l(printfa.o)
    0x00010f60   0x00010f60   0x00000024   Code   RO         2104    i.__0vsprintf       mc_p.l(printfa.o)
    0x00010f84   0x00010f84   0x0000002e   Code   RO         2184    i.__ARM_clz         mf_p.l(depilogue.o)
    0x00010fb2   0x00010fb2   0x0000001a   Code   RO          428    i.__ARM_common_switch8  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00010fcc   0x00010fcc   0x00000020   Code   RO         1524    i.__NVIC_DisableIRQ  CVWL668T.lib(drv_rxbr.o)
    0x00010fec   0x00010fec   0x0000000e   Code   RO         2196    i.__scatterload_copy  mc_p.l(handlers.o)
    0x00010ffa   0x00010ffa   0x00000002   Code   RO         2197    i.__scatterload_null  mc_p.l(handlers.o)
    0x00010ffc   0x00010ffc   0x00000004   PAD
    0x00011000   0x00011000   0x0000001c   Data   RO          884    .ARM.__at_0x11000   CVWL668T.lib(drv_common.o)
    0x0001101c   0x0001101c   0x00000010   Data   RO          677    .ARM.__at_0x1101C   CVWL668T.lib(tau_log.o)
    0x0001102c   0x0001102c   0x00000016   Data   RO          481    .ARM.__at_0x1102C   CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00011042   0x00011042   0x00000002   PAD
    0x00011044   0x00011044   0x00000364   Code   RO         1202    i.MIPI_RX_IRQn_Handler  CVWL668T.lib(drv_dsi_rx.o)
    0x000113a8   0x000113a8   0x00000180   Code   RO         1760    i.UART_IRQn_Handler  CVWL668T.lib(drv_uart.o)
    0x00011528   0x00011528   0x00000018   Code   RO         1525    i.__NVIC_EnableIRQ  CVWL668T.lib(drv_rxbr.o)
    0x00011540   0x00011540   0x0000000e   Code   RO         2198    i.__scatterload_zeroinit  mc_p.l(handlers.o)
    0x0001154e   0x0001154e   0x00000002   PAD
    0x00011550   0x00011550   0x00000174   Code   RO         2105    i._fp_digits        mc_p.l(printfa.o)
    0x000116c4   0x000116c4   0x000006ec   Code   RO         2106    i._printf_core      mc_p.l(printfa.o)
    0x00011db0   0x00011db0   0x00000020   Code   RO         2107    i._printf_post_padding  mc_p.l(printfa.o)
    0x00011dd0   0x00011dd0   0x0000002c   Code   RO         2108    i._printf_pre_padding  mc_p.l(printfa.o)
    0x00011dfc   0x00011dfc   0x0000000a   Code   RO         2110    i._sputc            mc_p.l(printfa.o)
    0x00011e06   0x00011e06   0x00000002   PAD
    0x00011e08   0x00011e08   0x00000144   Code   RO           94    i.ap_dcs_read       p6a_demo.o
    0x00011f4c   0x00011f4c   0x000000a4   Code   RO           95    i.ap_dcs_set_backlight  p6a_demo.o
    0x00011ff0   0x00011ff0   0x00000048   Code   RO           96    i.ap_dcs_set_display_off  p6a_demo.o
    0x00012038   0x00012038   0x00000044   Code   RO           97    i.ap_dcs_set_display_on  p6a_demo.o
    0x0001207c   0x0001207c   0x00000060   Code   RO           98    i.ap_dcs_set_enter_sleep_mode  p6a_demo.o
    0x000120dc   0x000120dc   0x00000040   Code   RO          100    i.ap_dcs_set_exit_sleep_mode  p6a_demo.o
    0x0001211c   0x0001211c   0x0000001e   Code   RO          105    i.app_display_init  p6a_demo.o
    0x0001213a   0x0001213a   0x00000002   PAD
    0x0001213c   0x0001213c   0x0000001c   Code   RO          106    i.app_gpio_init     p6a_demo.o
    0x00012158   0x00012158   0x00000018   Code   RO          107    i.app_init_panel    p6a_demo.o
    0x00012170   0x00012170   0x0000012c   Code   RO          108    i.app_mipi_rx_init  p6a_demo.o
    0x0001229c   0x0001229c   0x000000f8   Code   RO          109    i.app_mipi_tx_init  p6a_demo.o
    0x00012394   0x00012394   0x0000008c   Code   RO          110    i.app_mipi_tx_start  p6a_demo.o
    0x00012420   0x00012420   0x0000002e   Code   RO          114    i.app_tx_panel_reset  p6a_demo.o
    0x0001244e   0x0001244e   0x00000002   PAD
    0x00012450   0x00012450   0x00000018   Code   RO          307    i.board_Init        board.o
    0x00012468   0x00012468   0x000000c8   Code   RO         1845    i.ceil              m_ps.l(ceil.o)
    0x00012530   0x00012530   0x0000002c   Code   RO          722    i.check_mipi_rx_tx_video_info  CVWL668T.lib(hal_internal_vsync.o)
    0x0001255c   0x0001255c   0x00000088   Code   RO          788    i.check_pkt_buf_rev  CVWL668T.lib(hal_internal_dcs.o)
    0x000125e4   0x000125e4   0x00000058   Code   RO         1168    i.dcs_packet_fifo_alloc  CVWL668T.lib(dcs_packet_fifo.o)
    0x0001263c   0x0001263c   0x00000018   Code   RO         1169    i.dcs_packet_fifo_init  CVWL668T.lib(dcs_packet_fifo.o)
    0x00012654   0x00012654   0x00000044   Code   RO         1170    i.dcs_packet_free_fifo_header  CVWL668T.lib(dcs_packet_fifo.o)
    0x00012698   0x00012698   0x00000024   Code   RO         1171    i.dcs_packet_get_fifo_header  CVWL668T.lib(dcs_packet_fifo.o)
    0x000126bc   0x000126bc   0x00000018   Code   RO          664    i.delayMs           CVWL668T.lib(tau_delay.o)
    0x000126d4   0x000126d4   0x0000002c   Code   RO          665    i.delayUs           CVWL668T.lib(tau_delay.o)
    0x00012700   0x00012700   0x00000008   Code   RO          882    i.drv_common_system_init  CVWL668T.lib(drv_common.o)
    0x00012708   0x00012708   0x0000003c   Code   RO          901    i.drv_crgu_enable_clock  CVWL668T.lib(drv_crgu.o)
    0x00012744   0x00012744   0x00000068   Code   RO          904    i.drv_crgu_get_rxbr_clk  CVWL668T.lib(drv_crgu.o)
    0x000127ac   0x000127ac   0x00000028   Code   RO          908    i.drv_crgu_set_ahb_clk  CVWL668T.lib(drv_crgu.o)
    0x000127d4   0x000127d4   0x0000003c   Code   RO          911    i.drv_crgu_set_dpi_clk  CVWL668T.lib(drv_crgu.o)
    0x00012810   0x00012810   0x00000038   Code   RO          912    i.drv_crgu_set_dsc_clk  CVWL668T.lib(drv_crgu.o)
    0x00012848   0x00012848   0x00000028   Code   RO          913    i.drv_crgu_set_fb_clk  CVWL668T.lib(drv_crgu.o)
    0x00012870   0x00012870   0x00000028   Code   RO          914    i.drv_crgu_set_lcdc_clk  CVWL668T.lib(drv_crgu.o)
    0x00012898   0x00012898   0x00000018   Code   RO          915    i.drv_crgu_set_reset  CVWL668T.lib(drv_crgu.o)
    0x000128b0   0x000128b0   0x00000028   Code   RO          916    i.drv_crgu_set_rxbr_clk  CVWL668T.lib(drv_crgu.o)
    0x000128d8   0x000128d8   0x00000028   Code   RO          917    i.drv_crgu_set_vidc_clk  CVWL668T.lib(drv_crgu.o)
    0x00012900   0x00012900   0x00000018   Code   RO         1699    i.drv_dma_clear_status  CVWL668T.lib(drv_dma.o)
    0x00012918   0x00012918   0x00000014   Code   RO         1705    i.drv_dma_get_int_source  CVWL668T.lib(drv_dma.o)
    0x0001292c   0x0001292c   0x00000038   Code   RO          942    i.drv_dsc_dec_enable  CVWL668T.lib(drv_dsc_dec.o)
    0x00012964   0x00012964   0x00000020   Code   RO          943    i.drv_dsc_dec_get_nslc  CVWL668T.lib(drv_dsc_dec.o)
    0x00012984   0x00012984   0x0000001c   Code   RO          944    i.drv_dsc_dec_set_irqen  CVWL668T.lib(drv_dsc_dec.o)
    0x000129a0   0x000129a0   0x0000010c   Code   RO         1203    i.drv_dsi_rx_calc_ipi_tx_delay  CVWL668T.lib(drv_dsi_rx.o)
    0x00012aac   0x00012aac   0x00000040   Code   RO         1204    i.drv_dsi_rx_enable_irq  CVWL668T.lib(drv_dsi_rx.o)
    0x00012aec   0x00012aec   0x00000050   Code   RO         1206    i.drv_dsi_rx_get_color_bpp  CVWL668T.lib(drv_dsi_rx.o)
    0x00012b3c   0x00012b3c   0x0000001c   Code   RO         1207    i.drv_dsi_rx_get_color_pcc  CVWL668T.lib(drv_dsi_rx.o)
    0x00012b58   0x00012b58   0x00000010   Code   RO         1208    i.drv_dsi_rx_get_compression_en  CVWL668T.lib(drv_dsi_rx.o)
    0x00012b68   0x00012b68   0x00000010   Code   RO         1209    i.drv_dsi_rx_get_ddi_crc_en  CVWL668T.lib(drv_dsi_rx.o)
    0x00012b78   0x00012b78   0x0000000c   Code   RO         1211    i.drv_dsi_rx_get_max_ret_size  CVWL668T.lib(drv_dsi_rx.o)
    0x00012b84   0x00012b84   0x00000018   Code   RO         1214    i.drv_dsi_rx_power_up  CVWL668T.lib(drv_dsi_rx.o)
    0x00012b9c   0x00012b9c   0x0000001c   Code   RO         1215    i.drv_dsi_rx_set_check_crc  CVWL668T.lib(drv_dsi_rx.o)
    0x00012bb8   0x00012bb8   0x00000024   Code   RO         1216    i.drv_dsi_rx_set_ctrl_cfg  CVWL668T.lib(drv_dsi_rx.o)
    0x00012bdc   0x00012bdc   0x00000010   Code   RO         1217    i.drv_dsi_rx_set_ddi_cfg  CVWL668T.lib(drv_dsi_rx.o)
    0x00012bec   0x00012bec   0x0000001c   Code   RO         1218    i.drv_dsi_rx_set_ddi_crc_en  CVWL668T.lib(drv_dsi_rx.o)
    0x00012c08   0x00012c08   0x0000000c   Code   RO         1221    i.drv_dsi_rx_set_inten  CVWL668T.lib(drv_dsi_rx.o)
    0x00012c14   0x00012c14   0x00000010   Code   RO         1222    i.drv_dsi_rx_set_ipi_cfg  CVWL668T.lib(drv_dsi_rx.o)
    0x00012c24   0x00012c24   0x0000001c   Code   RO         1224    i.drv_dsi_rx_set_ipi_ycbcr_frmt  CVWL668T.lib(drv_dsi_rx.o)
    0x00012c40   0x00012c40   0x00000014   Code   RO         1225    i.drv_dsi_rx_set_lane_swap  CVWL668T.lib(drv_dsi_rx.o)
    0x00012c54   0x00012c54   0x00000024   Code   RO         1226    i.drv_dsi_rx_set_resp_cnt  CVWL668T.lib(drv_dsi_rx.o)
    0x00012c78   0x00012c78   0x0000001c   Code   RO         1227    i.drv_dsi_rx_set_tear_resp_en  CVWL668T.lib(drv_dsi_rx.o)
    0x00012c94   0x00012c94   0x00000100   Code   RO         1228    i.drv_dsi_rx_set_up_phy  CVWL668T.lib(drv_dsi_rx.o)
    0x00012d94   0x00012d94   0x00000018   Code   RO         1265    i.drv_dsi_tx_command_header  CVWL668T.lib(drv_dsi_tx.o)
    0x00012dac   0x00012dac   0x00000058   Code   RO         1266    i.drv_dsi_tx_command_mode_cfg  CVWL668T.lib(drv_dsi_tx.o)
    0x00012e04   0x00012e04   0x0000000c   Code   RO         1267    i.drv_dsi_tx_command_put_payload  CVWL668T.lib(drv_dsi_tx.o)
    0x00012e10   0x00012e10   0x00000020   Code   RO         1268    i.drv_dsi_tx_config_eotp  CVWL668T.lib(drv_dsi_tx.o)
    0x00012e30   0x00012e30   0x0000000c   Code   RO         1269    i.drv_dsi_tx_config_int  CVWL668T.lib(drv_dsi_tx.o)
    0x00012e3c   0x00012e3c   0x00000010   Code   RO         1270    i.drv_dsi_tx_dpi_lpcmd_time  CVWL668T.lib(drv_dsi_tx.o)
    0x00012e4c   0x00012e4c   0x00000010   Code   RO         1271    i.drv_dsi_tx_dpi_mode  CVWL668T.lib(drv_dsi_tx.o)
    0x00012e5c   0x00012e5c   0x00000024   Code   RO         1272    i.drv_dsi_tx_dpi_polarity  CVWL668T.lib(drv_dsi_tx.o)
    0x00012e80   0x00012e80   0x0000000c   Code   RO         1273    i.drv_dsi_tx_edpi_cmd_size  CVWL668T.lib(drv_dsi_tx.o)
    0x00012e8c   0x00012e8c   0x0000000c   Code   RO         1275    i.drv_dsi_tx_get_cmd_status  CVWL668T.lib(drv_dsi_tx.o)
    0x00012e98   0x00012e98   0x0000000c   Code   RO         1277    i.drv_dsi_tx_mode   CVWL668T.lib(drv_dsi_tx.o)
    0x00012ea4   0x00012ea4   0x0000001c   Code   RO         1278    i.drv_dsi_tx_phy_clock_lane_auto_lp  CVWL668T.lib(drv_dsi_tx.o)
    0x00012ec0   0x00012ec0   0x00000020   Code   RO         1279    i.drv_dsi_tx_phy_clock_lane_req_hs  CVWL668T.lib(drv_dsi_tx.o)
    0x00012ee0   0x00012ee0   0x00000010   Code   RO         1281    i.drv_dsi_tx_phy_lane_mode  CVWL668T.lib(drv_dsi_tx.o)
    0x00012ef0   0x00012ef0   0x00000068   Code   RO         1284    i.drv_dsi_tx_phy_status_ready  CVWL668T.lib(drv_dsi_tx.o)
    0x00012f58   0x00012f58   0x00000044   Code   RO         1285    i.drv_dsi_tx_phy_status_stopstate  CVWL668T.lib(drv_dsi_tx.o)
    0x00012f9c   0x00012f9c   0x00000150   Code   RO         1287    i.drv_dsi_tx_phy_test_setup  CVWL668T.lib(drv_dsi_tx.o)
    0x000130ec   0x000130ec   0x00000020   Code   RO         1288    i.drv_dsi_tx_phy_time_cfg  CVWL668T.lib(drv_dsi_tx.o)
    0x0001310c   0x0001310c   0x0000000c   Code   RO         1292    i.drv_dsi_tx_powerup  CVWL668T.lib(drv_dsi_tx.o)
    0x00013118   0x00013118   0x00000024   Code   RO         1293    i.drv_dsi_tx_response_mode  CVWL668T.lib(drv_dsi_tx.o)
    0x0001313c   0x0001313c   0x0000001c   Code   RO         1296    i.drv_dsi_tx_set_bta_ack  CVWL668T.lib(drv_dsi_tx.o)
    0x00013158   0x00013158   0x00000014   Code   RO         1297    i.drv_dsi_tx_set_esc_div  CVWL668T.lib(drv_dsi_tx.o)
    0x0001316c   0x0001316c   0x00000040   Code   RO         1298    i.drv_dsi_tx_set_int  CVWL668T.lib(drv_dsi_tx.o)
    0x000131ac   0x000131ac   0x00000018   Code   RO         1299    i.drv_dsi_tx_set_time_out_div  CVWL668T.lib(drv_dsi_tx.o)
    0x000131c4   0x000131c4   0x00000014   Code   RO         1300    i.drv_dsi_tx_set_video_chunk  CVWL668T.lib(drv_dsi_tx.o)
    0x000131d8   0x000131d8   0x00000024   Code   RO         1301    i.drv_dsi_tx_set_video_timing  CVWL668T.lib(drv_dsi_tx.o)
    0x000131fc   0x000131fc   0x0000000c   Code   RO         1303    i.drv_dsi_tx_shutdown  CVWL668T.lib(drv_dsi_tx.o)
    0x00013208   0x00013208   0x0000002c   Code   RO         1304    i.drv_dsi_tx_timeout_cfg  CVWL668T.lib(drv_dsi_tx.o)
    0x00013234   0x00013234   0x000000e8   Code   RO         1307    i.drv_dsi_tx_video_mode_cfg  CVWL668T.lib(drv_dsi_tx.o)
    0x0001331c   0x0001331c   0x00000036   Code   RO         1805    i.drv_efuse_enter_inactive  CVWL668T.lib(drv_efuse.o)
    0x00013352   0x00013352   0x0000000c   Code   RO         1808    i.drv_efuse_int_enable  CVWL668T.lib(drv_efuse.o)
    0x0001335e   0x0001335e   0x0000003a   Code   RO         1809    i.drv_efuse_read    CVWL668T.lib(drv_efuse.o)
    0x00013398   0x00013398   0x00000018   Code   RO         1810    i.drv_efuse_read_req  CVWL668T.lib(drv_efuse.o)
    0x000133b0   0x000133b0   0x00000024   Code   RO          964    i.drv_gpio_handle_int  CVWL668T.lib(drv_gpio.o)
    0x000133d4   0x000133d4   0x00000020   Code   RO          969    i.drv_gpio_set_ioe  CVWL668T.lib(drv_gpio.o)
    0x000133f4   0x000133f4   0x00000014   Code   RO          970    i.drv_gpio_set_mode  CVWL668T.lib(drv_gpio.o)
    0x00013408   0x00013408   0x00000020   Code   RO          538    i.drv_gpio_set_output_data  CVWL668T.lib(hal_gpio.o)
    0x00013428   0x00013428   0x00000028   Code   RO         1369    i.drv_lcdc_bcsa_config  CVWL668T.lib(drv_lcdc.o)
    0x00013450   0x00013450   0x0000002c   Code   RO         1370    i.drv_lcdc_cfg_int_frame  CVWL668T.lib(drv_lcdc.o)
    0x0001347c   0x0001347c   0x00000018   Code   RO         1371    i.drv_lcdc_clear_int  CVWL668T.lib(drv_lcdc.o)
    0x00013494   0x00013494   0x00000034   Code   RO         1373    i.drv_lcdc_cmd_start  CVWL668T.lib(drv_lcdc.o)
    0x000134c8   0x000134c8   0x00000014   Code   RO         1374    i.drv_lcdc_config_acc_command_mode  CVWL668T.lib(drv_lcdc.o)
    0x000134dc   0x000134dc   0x00000038   Code   RO         1375    i.drv_lcdc_config_int  CVWL668T.lib(drv_lcdc.o)
    0x00013514   0x00013514   0x00000028   Code   RO         1376    i.drv_lcdc_config_int_single  CVWL668T.lib(drv_lcdc.o)
    0x0001353c   0x0001353c   0x00000018   Code   RO         1377    i.drv_lcdc_config_overwrite_rgb  CVWL668T.lib(drv_lcdc.o)
    0x00013554   0x00013554   0x00000050   Code   RO         1378    i.drv_lcdc_config_src_parameter  CVWL668T.lib(drv_lcdc.o)
    0x000135a4   0x000135a4   0x00000010   Code   RO         1379    i.drv_lcdc_crop_hact  CVWL668T.lib(drv_lcdc.o)
    0x000135b4   0x000135b4   0x00000038   Code   RO         1380    i.drv_lcdc_ctrl_flow  CVWL668T.lib(drv_lcdc.o)
    0x000135ec   0x000135ec   0x00000030   Code   RO         1381    i.drv_lcdc_dith_config  CVWL668T.lib(drv_lcdc.o)
    0x0001361c   0x0001361c   0x0000003c   Code   RO         1383    i.drv_lcdc_edge_dect_config  CVWL668T.lib(drv_lcdc.o)
    0x00013658   0x00013658   0x00000064   Code   RO         1384    i.drv_lcdc_edge_enh_config  CVWL668T.lib(drv_lcdc.o)
    0x000136bc   0x000136bc   0x00000024   Code   RO         1385    i.drv_lcdc_enable_shadow_reg  CVWL668T.lib(drv_lcdc.o)
    0x000136e0   0x000136e0   0x0000001c   Code   RO         1386    i.drv_lcdc_endianness_config  CVWL668T.lib(drv_lcdc.o)
    0x000136fc   0x000136fc   0x00000020   Code   RO         1387    i.drv_lcdc_fc_config  CVWL668T.lib(drv_lcdc.o)
    0x0001371c   0x0001371c   0x00000024   Code   RO         1389    i.drv_lcdc_fldc_config  CVWL668T.lib(drv_lcdc.o)
    0x00013740   0x00013740   0x00000024   Code   RO         1390    i.drv_lcdc_function_disable  CVWL668T.lib(drv_lcdc.o)
    0x00013764   0x00013764   0x00000024   Code   RO         1391    i.drv_lcdc_function_enable  CVWL668T.lib(drv_lcdc.o)
    0x00013788   0x00013788   0x0000003c   Code   RO         1402    i.drv_lcdc_set_int  CVWL668T.lib(drv_lcdc.o)
    0x000137c4   0x000137c4   0x0000001c   Code   RO         1403    i.drv_lcdc_set_prefetch  CVWL668T.lib(drv_lcdc.o)
    0x000137e0   0x000137e0   0x0000001c   Code   RO         1404    i.drv_lcdc_set_tear_line  CVWL668T.lib(drv_lcdc.o)
    0x000137fc   0x000137fc   0x0000003c   Code   RO         1408    i.drv_lcdc_vid_hw_start  CVWL668T.lib(drv_lcdc.o)
    0x00013838   0x00013838   0x00000018   Code   RO         1410    i.drv_lcdc_vintp_mode_config  CVWL668T.lib(drv_lcdc.o)
    0x00013850   0x00013850   0x00000014   Code   RO         1458    i.drv_memc_clear_status  CVWL668T.lib(drv_memc.o)
    0x00013864   0x00013864   0x00000040   Code   RO         1459    i.drv_memc_enable_irq  CVWL668T.lib(drv_memc.o)
    0x000138a4   0x000138a4   0x00000010   Code   RO         1460    i.drv_memc_gen_a_tear_signal  CVWL668T.lib(drv_memc.o)
    0x000138b4   0x000138b4   0x00000018   Code   RO         1461    i.drv_memc_get_status  CVWL668T.lib(drv_memc.o)
    0x000138cc   0x000138cc   0x00000010   Code   RO         1462    i.drv_memc_get_tear_mode  CVWL668T.lib(drv_memc.o)
    0x000138dc   0x000138dc   0x0000001c   Code   RO         1463    i.drv_memc_rate_transfer_sel  CVWL668T.lib(drv_memc.o)
    0x000138f8   0x000138f8   0x00000014   Code   RO         1464    i.drv_memc_sel_vsync  CVWL668T.lib(drv_memc.o)
    0x0001390c   0x0001390c   0x00000018   Code   RO         1465    i.drv_memc_set_active_height  CVWL668T.lib(drv_memc.o)
    0x00013924   0x00013924   0x0000001c   Code   RO         1466    i.drv_memc_set_circ_mode_enable  CVWL668T.lib(drv_memc.o)
    0x00013940   0x00013940   0x00000014   Code   RO         1467    i.drv_memc_set_data_mode  CVWL668T.lib(drv_memc.o)
    0x00013954   0x00013954   0x00000018   Code   RO         1470    i.drv_memc_set_double_buffer  CVWL668T.lib(drv_memc.o)
    0x0001396c   0x0001396c   0x0000001c   Code   RO         1474    i.drv_memc_set_frame_drop_select  CVWL668T.lib(drv_memc.o)
    0x00013988   0x00013988   0x00000018   Code   RO         1475    i.drv_memc_set_fs_en_conditions  CVWL668T.lib(drv_memc.o)
    0x000139a0   0x000139a0   0x0000001c   Code   RO         1477    i.drv_memc_set_lcdc_st_conditions  CVWL668T.lib(drv_memc.o)
    0x000139bc   0x000139bc   0x00000020   Code   RO         1478    i.drv_memc_set_ltpo_mode  CVWL668T.lib(drv_memc.o)
    0x000139dc   0x000139dc   0x00000018   Code   RO         1479    i.drv_memc_set_ltpo_pu_thres  CVWL668T.lib(drv_memc.o)
    0x000139f4   0x000139f4   0x00000014   Code   RO         1483    i.drv_memc_set_tear_mode  CVWL668T.lib(drv_memc.o)
    0x00013a08   0x00013a08   0x0000002c   Code   RO         1484    i.drv_memc_set_tear_waveform  CVWL668T.lib(drv_memc.o)
    0x00013a34   0x00013a34   0x00000014   Code   RO         1486    i.drv_memc_set_vidc_sync_cnt  CVWL668T.lib(drv_memc.o)
    0x00013a48   0x00013a48   0x00000010   Code   RO         1828    i.drv_phy_test_clear  CVWL668T.lib(drv_phy_common.o)
    0x00013a58   0x00013a58   0x00000018   Code   RO         1829    i.drv_phy_test_lock  CVWL668T.lib(drv_phy_common.o)
    0x00013a70   0x00013a70   0x00000030   Code   RO         1000    i.drv_pwr_efuse_pd  CVWL668T.lib(drv_pwr.o)
    0x00013aa0   0x00013aa0   0x00000010   Code   RO         1009    i.drv_pwr_get_power_ready_st  CVWL668T.lib(drv_pwr.o)
    0x00013ab0   0x00013ab0   0x00000028   Code   RO         1042    i.drv_pwr_set_digit_power_sel  CVWL668T.lib(drv_pwr.o)
    0x00013ad8   0x00013ad8   0x00000034   Code   RO         1045    i.drv_pwr_set_pll_clk  CVWL668T.lib(drv_pwr.o)
    0x00013b0c   0x00013b0c   0x00000020   Code   RO         1052    i.drv_pwr_write_lock  CVWL668T.lib(drv_pwr.o)
    0x00013b2c   0x00013b2c   0x00000010   Code   RO         1526    i.drv_rxbr_clear_pkt_buffer  CVWL668T.lib(drv_rxbr.o)
    0x00013b3c   0x00013b3c   0x0000000c   Code   RO         1527    i.drv_rxbr_clear_status0  CVWL668T.lib(drv_rxbr.o)
    0x00013b48   0x00013b48   0x0000005a   Code   RO         1530    i.drv_rxbr_enable_irq  CVWL668T.lib(drv_rxbr.o)
    0x00013ba2   0x00013ba2   0x00000002   PAD
    0x00013ba4   0x00013ba4   0x0000001c   Code   RO         1531    i.drv_rxbr_frame_drop_cfg  CVWL668T.lib(drv_rxbr.o)
    0x00013bc0   0x00013bc0   0x00000018   Code   RO          723    i.drv_rxbr_get_int_source  CVWL668T.lib(hal_internal_vsync.o)
    0x00013bd8   0x00013bd8   0x00000018   Code   RO          789    i.drv_rxbr_get_status0  CVWL668T.lib(hal_internal_dcs.o)
    0x00013bf0   0x00013bf0   0x00000014   Code   RO         1541    i.drv_rxbr_hline_rcv1_cfg  CVWL668T.lib(drv_rxbr.o)
    0x00013c04   0x00013c04   0x00000010   Code   RO         1542    i.drv_rxbr_hline_rcv_cfg  CVWL668T.lib(drv_rxbr.o)
    0x00013c14   0x00013c14   0x0000000c   Code   RO         1544    i.drv_rxbr_register_irq1_callback  CVWL668T.lib(drv_rxbr.o)
    0x00013c20   0x00013c20   0x00000018   Code   RO         1545    i.drv_rxbr_set_ack_pkt_header  CVWL668T.lib(drv_rxbr.o)
    0x00013c38   0x00013c38   0x0000001c   Code   RO         1550    i.drv_rxbr_set_color_format  CVWL668T.lib(drv_rxbr.o)
    0x00013c54   0x00013c54   0x00000024   Code   RO         1553    i.drv_rxbr_set_filter_regs  CVWL668T.lib(drv_rxbr.o)
    0x00013c78   0x00013c78   0x0000001c   Code   RO         1554    i.drv_rxbr_set_inten  CVWL668T.lib(drv_rxbr.o)
    0x00013c94   0x00013c94   0x00000018   Code   RO         1555    i.drv_rxbr_set_ltpo_drop_th  CVWL668T.lib(drv_rxbr.o)
    0x00013cac   0x00013cac   0x00000040   Code   RO         1559    i.drv_rxbr_set_usr_cfg  CVWL668T.lib(drv_rxbr.o)
    0x00013cec   0x00013cec   0x00000010   Code   RO         1560    i.drv_rxbr_set_usr_col  CVWL668T.lib(drv_rxbr.o)
    0x00013cfc   0x00013cfc   0x00000010   Code   RO         1561    i.drv_rxbr_set_usr_row  CVWL668T.lib(drv_rxbr.o)
    0x00013d0c   0x00013d0c   0x00000078   Code   RO         1183    i.drv_se_init       CVWL668T.lib(drv_se.o)
    0x00013d84   0x00013d84   0x000000d4   Code   RO         1184    i.drv_se_set_dsc    CVWL668T.lib(drv_se.o)
    0x00013e58   0x00013e58   0x00000088   Code   RO         1185    i.drv_se_set_lcdc   CVWL668T.lib(drv_se.o)
    0x00013ee0   0x00013ee0   0x00000068   Code   RO         1186    i.drv_se_set_memc   CVWL668T.lib(drv_se.o)
    0x00013f48   0x00013f48   0x000000d0   Code   RO         1187    i.drv_se_set_rxbr   CVWL668T.lib(drv_se.o)
    0x00014018   0x00014018   0x000000ac   Code   RO         1188    i.drv_se_set_vidc   CVWL668T.lib(drv_se.o)
    0x000140c4   0x000140c4   0x00000014   Code   RO         1189    i.drv_se_start_rx   CVWL668T.lib(drv_se.o)
    0x000140d8   0x000140d8   0x0000000c   Code   RO         1115    i.drv_sys_cfg_clear_all_int  CVWL668T.lib(drv_sys_cfg.o)
    0x000140e4   0x000140e4   0x00000028   Code   RO         1116    i.drv_sys_cfg_clear_pending  CVWL668T.lib(drv_sys_cfg.o)
    0x0001410c   0x0001410c   0x00000024   Code   RO         1122    i.drv_sys_cfg_set_int  CVWL668T.lib(drv_sys_cfg.o)
    0x00014130   0x00014130   0x0000001a   Code   RO         1139    i.drv_timer_clear_status_flags  CVWL668T.lib(drv_timer.o)
    0x0001414a   0x0001414a   0x00000020   Code   RO         1140    i.drv_timer_enable  CVWL668T.lib(drv_timer.o)
    0x0001416a   0x0001416a   0x00000002   PAD
    0x0001416c   0x0001416c   0x00000010   Code   RO         1141    i.drv_timer_get_instance  CVWL668T.lib(drv_timer.o)
    0x0001417c   0x0001417c   0x0000003c   Code   RO         1143    i.drv_timer_handle_interrupt  CVWL668T.lib(drv_timer.o)
    0x000141b8   0x000141b8   0x00000014   Code   RO         1144    i.drv_timer_register_callback  CVWL668T.lib(drv_timer.o)
    0x000141cc   0x000141cc   0x00000040   Code   RO         1145    i.drv_timer_set_compare_val  CVWL668T.lib(drv_timer.o)
    0x0001420c   0x0001420c   0x00000048   Code   RO         1146    i.drv_timer_set_int  CVWL668T.lib(drv_timer.o)
    0x00014254   0x00014254   0x00000028   Code   RO         1147    i.drv_timer_set_prescaler  CVWL668T.lib(drv_timer.o)
    0x0001427c   0x0001427c   0x00000010   Code   RO         1148    i.drv_timer_set_repeat  CVWL668T.lib(drv_timer.o)
    0x0001428c   0x0001428c   0x00000020   Code   RO         1309    i.drv_tx_phy_test_enter  CVWL668T.lib(drv_dsi_tx.o)
    0x000142ac   0x000142ac   0x00000020   Code   RO         1310    i.drv_tx_phy_test_exit  CVWL668T.lib(drv_dsi_tx.o)
    0x000142cc   0x000142cc   0x00000028   Code   RO         1313    i.drv_tx_phy_test_write_code  CVWL668T.lib(drv_dsi_tx.o)
    0x000142f4   0x000142f4   0x00000034   Code   RO         1761    i.drv_uart_abort_recv  CVWL668T.lib(drv_uart.o)
    0x00014328   0x00014328   0x00000034   Code   RO         1762    i.drv_uart_abort_send  CVWL668T.lib(drv_uart.o)
    0x0001435c   0x0001435c   0x00000014   Code   RO         1763    i.drv_uart_config_int  CVWL668T.lib(drv_uart.o)
    0x00014370   0x00014370   0x00000018   Code   RO         1765    i.drv_uart_enable_clk  CVWL668T.lib(drv_uart.o)
    0x00014388   0x00014388   0x0000005c   Code   RO         1766    i.drv_uart_enable_int  CVWL668T.lib(drv_uart.o)
    0x000143e4   0x000143e4   0x00000028   Code   RO         1768    i.drv_uart_get_instance  CVWL668T.lib(drv_uart.o)
    0x0001440c   0x0001440c   0x000000ce   Code   RO         1769    i.drv_uart_init     CVWL668T.lib(drv_uart.o)
    0x000144da   0x000144da   0x00000002   PAD
    0x000144dc   0x000144dc   0x0000003c   Code   RO         1770    i.drv_uart_int_trans_handle  CVWL668T.lib(drv_uart.o)
    0x00014518   0x00014518   0x0000001c   Code   RO         1773    i.drv_uart_reset_rx_fifo  CVWL668T.lib(drv_uart.o)
    0x00014534   0x00014534   0x0000001c   Code   RO         1774    i.drv_uart_reset_tx_fifo  CVWL668T.lib(drv_uart.o)
    0x00014550   0x00014550   0x0000001a   Code   RO         1775    i.drv_uart_send_blocking  CVWL668T.lib(drv_uart.o)
    0x0001456a   0x0001456a   0x00000054   Code   RO         1777    i.drv_uart_set_baud_rate  CVWL668T.lib(drv_uart.o)
    0x000145be   0x000145be   0x00000002   PAD
    0x000145c0   0x000145c0   0x0000004c   Code   RO         1778    i.drv_uart_trans_create_handle  CVWL668T.lib(drv_uart.o)
    0x0001460c   0x0001460c   0x00000010   Code   RO         1613    i.drv_vidc_clear_irq  CVWL668T.lib(drv_vidc.o)
    0x0001461c   0x0001461c   0x00000020   Code   RO         1617    i.drv_vidc_enable   CVWL668T.lib(drv_vidc.o)
    0x0001463c   0x0001463c   0x00000040   Code   RO         1618    i.drv_vidc_enable_irq  CVWL668T.lib(drv_vidc.o)
    0x0001467c   0x0001467c   0x0000002c   Code   RO         1619    i.drv_vidc_get_int_source  CVWL668T.lib(drv_vidc.o)
    0x000146a8   0x000146a8   0x00000018   Code   RO         1620    i.drv_vidc_get_irq_status  CVWL668T.lib(drv_vidc.o)
    0x000146c0   0x000146c0   0x0000002c   Code   RO         1624    i.drv_vidc_init_module_enable  CVWL668T.lib(drv_vidc.o)
    0x000146ec   0x000146ec   0x0000000c   Code   RO         1625    i.drv_vidc_register_callback  CVWL668T.lib(drv_vidc.o)
    0x000146f8   0x000146f8   0x0000000c   Code   RO         1626    i.drv_vidc_reset    CVWL668T.lib(drv_vidc.o)
    0x00014704   0x00014704   0x0000001c   Code   RO         1627    i.drv_vidc_set_circ_mode_enable  CVWL668T.lib(drv_vidc.o)
    0x00014720   0x00014720   0x00000038   Code   RO         1628    i.drv_vidc_set_dither_config  CVWL668T.lib(drv_vidc.o)
    0x00014758   0x00014758   0x0000005c   Code   RO         1630    i.drv_vidc_set_dst_parameter  CVWL668T.lib(drv_vidc.o)
    0x000147b4   0x000147b4   0x0000000c   Code   RO         1632    i.drv_vidc_set_honly_hcoef0  CVWL668T.lib(drv_vidc.o)
    0x000147c0   0x000147c0   0x0000002c   Code   RO         1633    i.drv_vidc_set_honly_hinitb  CVWL668T.lib(drv_vidc.o)
    0x000147ec   0x000147ec   0x00000030   Code   RO         1634    i.drv_vidc_set_honly_hinitr  CVWL668T.lib(drv_vidc.o)
    0x0001481c   0x0001481c   0x0000001c   Code   RO         1637    i.drv_vidc_set_irqen  CVWL668T.lib(drv_vidc.o)
    0x00014838   0x00014838   0x00000014   Code   RO         1638    i.drv_vidc_set_mirror  CVWL668T.lib(drv_vidc.o)
    0x0001484c   0x0001484c   0x0000001c   Code   RO         1641    i.drv_vidc_set_pentile_swap  CVWL668T.lib(drv_vidc.o)
    0x00014868   0x00014868   0x0000000c   Code   RO         1642    i.drv_vidc_set_pu_ctrl  CVWL668T.lib(drv_vidc.o)
    0x00014874   0x00014874   0x00000018   Code   RO         1643    i.drv_vidc_set_rotation  CVWL668T.lib(drv_vidc.o)
    0x0001488c   0x0001488c   0x0000000c   Code   RO         1644    i.drv_vidc_set_scld_hcoef0  CVWL668T.lib(drv_vidc.o)
    0x00014898   0x00014898   0x0000000c   Code   RO         1645    i.drv_vidc_set_scld_hcoef1  CVWL668T.lib(drv_vidc.o)
    0x000148a4   0x000148a4   0x00000014   Code   RO         1646    i.drv_vidc_set_scld_step  CVWL668T.lib(drv_vidc.o)
    0x000148b8   0x000148b8   0x0000000c   Code   RO         1647    i.drv_vidc_set_scld_vcoef0  CVWL668T.lib(drv_vidc.o)
    0x000148c4   0x000148c4   0x0000000c   Code   RO         1648    i.drv_vidc_set_scld_vcoef1  CVWL668T.lib(drv_vidc.o)
    0x000148d0   0x000148d0   0x00000020   Code   RO         1649    i.drv_vidc_set_src_parameter  CVWL668T.lib(drv_vidc.o)
    0x000148f0   0x000148f0   0x00000038   Code   RO         1650    i.drv_vidc_set_vintp_config  CVWL668T.lib(drv_vidc.o)
    0x00014928   0x00014928   0x00000034   Code   RO          673    i.fputc             CVWL668T.lib(tau_log.o)
    0x0001495c   0x0001495c   0x0000005c   Code   RO          115    i.google_p6a_demo   p6a_demo.o
    0x000149b8   0x000149b8   0x00000040   Code   RO          817    i.ha_intl_fb_check_pu_size  CVWL668T.lib(hal_internal_fb.o)
    0x000149f8   0x000149f8   0x00000040   Code   RO          342    i.hal_dsi_rx_ctrl_create_handle  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00014a38   0x00014a38   0x00000040   Code   RO          343    i.hal_dsi_rx_ctrl_dcs_async_handler  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00014a78   0x00014a78   0x00000020   Code   RO          351    i.hal_dsi_rx_ctrl_get_max_ret_size  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00014a98   0x00014a98   0x000000ac   Code   RO          352    i.hal_dsi_rx_ctrl_init  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00014b44   0x00014b44   0x00000100   Code   RO          353    i.hal_dsi_rx_ctrl_init_clk  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00014c44   0x00014c44   0x00000108   Code   RO          354    i.hal_dsi_rx_ctrl_init_dsi_rx  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00014d4c   0x00014d4c   0x0000012c   Code   RO          355    i.hal_dsi_rx_ctrl_init_memc  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00014e78   0x00014e78   0x00000148   Code   RO          356    i.hal_dsi_rx_ctrl_init_rxbr  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00014fc0   0x00014fc0   0x00000280   Code   RO          357    i.hal_dsi_rx_ctrl_init_vidc  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00015240   0x00015240   0x00000038   Code   RO          358    i.hal_dsi_rx_ctrl_pre_init_pps  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00015278   0x00015278   0x000000f0   Code   RO          363    i.hal_dsi_rx_ctrl_send_ack_cmd  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00015368   0x00015368   0x00000030   Code   RO          370    i.hal_dsi_rx_ctrl_set_ipi_cfg  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00015398   0x00015398   0x00000030   Code   RO          376    i.hal_dsi_rx_ctrl_start  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x000153c8   0x000153c8   0x00000020   Code   RO          379    i.hal_dsi_rx_ctrl_toggle_resolution  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x000153e8   0x000153e8   0x00000280   Code   RO          432    i.hal_dsi_tx_cmd_mode_cal_timing  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00015668   0x00015668   0x00000038   Code   RO          434    i.hal_dsi_tx_ctrl_create_handle  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x000156a0   0x000156a0   0x00000022   Code   RO          438    i.hal_dsi_tx_ctrl_gen_a_tear_signal  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x000156c2   0x000156c2   0x00000002   PAD
    0x000156c4   0x000156c4   0x0000007c   Code   RO          440    i.hal_dsi_tx_ctrl_init  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00015740   0x00015740   0x00000010   Code   RO          441    i.hal_dsi_tx_ctrl_init_clk  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00015750   0x00015750   0x00000008   Code   RO          454    i.hal_dsi_tx_ctrl_set_overwrite_rgb  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00015758   0x00015758   0x0000000a   Code   RO          455    i.hal_dsi_tx_ctrl_set_tear_mode  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00015762   0x00015762   0x00000002   PAD
    0x00015764   0x00015764   0x00000090   Code   RO          457    i.hal_dsi_tx_ctrl_start  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x000157f4   0x000157f4   0x000000f4   Code   RO          460    i.hal_dsi_tx_ctrl_write_array_cmd  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x000158e8   0x000158e8   0x000000d0   Code   RO          461    i.hal_dsi_tx_ctrl_write_cmd  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x000159b8   0x000159b8   0x00000104   Code   RO          462    i.hal_dsi_tx_init_cfg  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00015abc   0x00015abc   0x00000044   Code   RO          463    i.hal_dsi_tx_init_dpi_timing  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00015b00   0x00015b00   0x00000016   Code   RO          464    i.hal_dsi_tx_init_phy_cfg  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00015b16   0x00015b16   0x00000052   Code   RO          465    i.hal_dsi_tx_init_timing  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00015b68   0x00015b68   0x00000054   Code   RO          466    i.hal_dsi_tx_init_vid_timing  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00015bbc   0x00015bbc   0x00000040   Code   RO          467    i.hal_dsi_tx_send_cmd  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00015bfc   0x00015bfc   0x00000094   Code   RO          468    i.hal_dsi_tx_timing_info_update  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00015c90   0x00015c90   0x00000310   Code   RO          469    i.hal_dsi_tx_vid_mode_cal_timing  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00015fa0   0x00015fa0   0x0000003a   Code   RO          539    i.hal_gpio_config_pad  CVWL668T.lib(hal_gpio.o)
    0x00015fda   0x00015fda   0x00000016   Code   RO          545    i.hal_gpio_init_input  CVWL668T.lib(hal_gpio.o)
    0x00015ff0   0x00015ff0   0x0000001c   Code   RO          546    i.hal_gpio_init_output  CVWL668T.lib(hal_gpio.o)
    0x0001600c   0x0001600c   0x00000060   Code   RO          551    i.hal_gpio_set_mode  CVWL668T.lib(hal_gpio.o)
    0x0001606c   0x0001606c   0x00000008   Code   RO          552    i.hal_gpio_set_output_data  CVWL668T.lib(hal_gpio.o)
    0x00016074   0x00016074   0x00000010   Code   RO          725    i.hal_internal_sync_get_hight_performan_mode  CVWL668T.lib(hal_internal_vsync.o)
    0x00016084   0x00016084   0x000001b4   Code   RO          726    i.hal_internal_sync_input_resolution_change  CVWL668T.lib(hal_internal_vsync.o)
    0x00016238   0x00016238   0x0000000c   Code   RO          727    i.hal_internal_sync_register_lcdc_cb  CVWL668T.lib(hal_internal_vsync.o)
    0x00016244   0x00016244   0x00000020   Code   RO          730    i.hal_internal_vsync_deinit  CVWL668T.lib(hal_internal_vsync.o)
    0x00016264   0x00016264   0x00000014   Code   RO          732    i.hal_internal_vsync_get_sync_line  CVWL668T.lib(hal_internal_vsync.o)
    0x00016278   0x00016278   0x0000000c   Code   RO          733    i.hal_internal_vsync_get_tx_state  CVWL668T.lib(hal_internal_vsync.o)
    0x00016284   0x00016284   0x000000e8   Code   RO          734    i.hal_internal_vsync_init_rx  CVWL668T.lib(hal_internal_vsync.o)
    0x0001636c   0x0001636c   0x000000c8   Code   RO          735    i.hal_internal_vsync_init_tx  CVWL668T.lib(hal_internal_vsync.o)
    0x00016434   0x00016434   0x00000020   Code   RO          736    i.hal_internal_vsync_set_rx_state  CVWL668T.lib(hal_internal_vsync.o)
    0x00016454   0x00016454   0x000001ec   Code   RO          738    i.hal_internal_vsync_set_tear_mode  CVWL668T.lib(hal_internal_vsync.o)
    0x00016640   0x00016640   0x00000058   Code   RO          739    i.hal_internal_vsync_set_tx_state  CVWL668T.lib(hal_internal_vsync.o)
    0x00016698   0x00016698   0x0000006c   Code   RO          790    i.hal_intl_dcs_init_sw_fltr  CVWL668T.lib(hal_internal_dcs.o)
    0x00016704   0x00016704   0x00000430   Code   RO          792    i.hal_intl_dcs_rx_get_dcs_packet_data  CVWL668T.lib(hal_internal_dcs.o)
    0x00016b34   0x00016b34   0x00000088   Code   RO          793    i.hal_intl_dcs_rx_receive_packet  CVWL668T.lib(hal_internal_dcs.o)
    0x00016bbc   0x00016bbc   0x00000174   Code   RO          794    i.hal_intl_dcs_rx_receive_pps  CVWL668T.lib(hal_internal_dcs.o)
    0x00016d30   0x00016d30   0x0000008c   Code   RO          795    i.hal_intl_dcs_set_auto_hw_filter  CVWL668T.lib(hal_internal_dcs.o)
    0x00016dbc   0x00016dbc   0x0000002c   Code   RO          797    i.hal_intl_dcs_sw_filter_handle  CVWL668T.lib(hal_internal_dcs.o)
    0x00016de8   0x00016de8   0x00000318   Code   RO          818    i.hal_intl_fb_cal_fb_info  CVWL668T.lib(hal_internal_fb.o)
    0x00017100   0x00017100   0x00000064   Code   RO          819    i.hal_intl_fb_check_bandwidth  CVWL668T.lib(hal_internal_fb.o)
    0x00017164   0x00017164   0x000000dc   Code   RO          820    i.hal_intl_fb_edge_resize  CVWL668T.lib(hal_internal_fb.o)
    0x00017240   0x00017240   0x00000074   Code   RO          821    i.hal_intl_fb_flow_control_adapter  CVWL668T.lib(hal_internal_fb.o)
    0x000172b4   0x000172b4   0x0000000c   Code   RO          822    i.hal_intl_fb_get_memc_flow_mode  CVWL668T.lib(hal_internal_fb.o)
    0x000172c0   0x000172c0   0x00000010   Code   RO          823    i.hal_intl_fb_get_rx_fb_info  CVWL668T.lib(hal_internal_fb.o)
    0x000172d0   0x000172d0   0x00000010   Code   RO          824    i.hal_intl_fb_get_tx_fb_info  CVWL668T.lib(hal_internal_fb.o)
    0x000172e0   0x000172e0   0x0000000c   Code   RO          825    i.hal_intl_fb_get_user_flow  CVWL668T.lib(hal_internal_fb.o)
    0x000172ec   0x000172ec   0x00000028   Code   RO          843    i.hal_intl_svs_deinit_rx  CVWL668T.lib(hal_internal_svs.o)
    0x00017314   0x00017314   0x00000010   Code   RO          844    i.hal_intl_svs_deinit_tx  CVWL668T.lib(hal_internal_svs.o)
    0x00017324   0x00017324   0x00000024   Code   RO          845    i.hal_intl_svs_handle  CVWL668T.lib(hal_internal_svs.o)
    0x00017348   0x00017348   0x00000080   Code   RO          846    i.hal_intl_svs_init_rx  CVWL668T.lib(hal_internal_svs.o)
    0x000173c8   0x000173c8   0x00000014   Code   RO          847    i.hal_intl_svs_init_tx  CVWL668T.lib(hal_internal_svs.o)
    0x000173dc   0x000173dc   0x0000000c   Code   RO          849    i.hal_intl_svs_set_rx_vtt  CVWL668T.lib(hal_internal_svs.o)
    0x000173e8   0x000173e8   0x00000048   Code   RO          851    i.hal_intl_svs_update_rxbr_clk  CVWL668T.lib(hal_internal_svs.o)
    0x00017430   0x00017430   0x00000070   Code   RO          470    i.hal_lcdc_displayproc_config  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x000174a0   0x000174a0   0x0000003e   Code   RO          471    i.hal_lcdc_init_cfg  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x000174de   0x000174de   0x00000070   Code   RO          472    i.hal_lcdc_init_clk  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001754e   0x0001754e   0x00000002   PAD
    0x00017550   0x00017550   0x00000128   Code   RO          473    i.hal_lcdc_postproc_config  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00017678   0x00017678   0x00000024   Code   RO          474    i.hal_lcdc_start    CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001769c   0x0001769c   0x0000003c   Code   RO          475    i.hal_lcdc_timinggen_config  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x000176d8   0x000176d8   0x000000e0   Code   RO          476    i.hal_lcdc_upscaler_config  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x000177b8   0x000177b8   0x000000bc   Code   RO          478    i.hal_nonshadow_func_update  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00017874   0x00017874   0x00000008   Code   RO          629    i.hal_pwr_get_vcc_power_ready  CVWL668T.lib(hal_pwr.o)
    0x0001787c   0x0001787c   0x00000008   Code   RO          634    i.hal_pwr_set_main_power  CVWL668T.lib(hal_pwr.o)
    0x00017884   0x00017884   0x000000e4   Code   RO          585    i.hal_system_init   CVWL668T.lib(hal_system.o)
    0x00017968   0x00017968   0x00000050   Code   RO          588    i.hal_system_updata_sysclk  CVWL668T.lib(hal_system.o)
    0x000179b8   0x000179b8   0x00000030   Code   RO          603    i.hal_timer_deinit  CVWL668T.lib(hal_timer.o)
    0x000179e8   0x000179e8   0x0000001c   Code   RO          605    i.hal_timer_init    CVWL668T.lib(hal_timer.o)
    0x00017a04   0x00017a04   0x00000030   Code   RO          607    i.hal_timer_start   CVWL668T.lib(hal_timer.o)
    0x00017a34   0x00017a34   0x00000028   Code   RO          609    i.hal_timer_stop    CVWL668T.lib(hal_timer.o)
    0x00017a5c   0x00017a5c   0x00000030   Code   RO          479    i.hal_tx_frame_rate_adjust  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00017a8c   0x00017a8c   0x00000094   Code   RO          697    i.hal_uart_init     CVWL668T.lib(hal_uart.o)
    0x00017b20   0x00017b20   0x0000001c   Code   RO          700    i.hal_uart_send_blocking  CVWL668T.lib(hal_uart.o)
    0x00017b3c   0x00017b3c   0x00000018   Code   RO          480    i.hal_vsync_func_update  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00017b54   0x00017b54   0x000000e0   Code   RO          741    i.hal_vsync_reset_lcdc_scaler  CVWL668T.lib(hal_internal_vsync.o)
    0x00017c34   0x00017c34   0x00000040   Code   RO            3    i.main              main.o
    0x00017c74   0x00017c74   0x00000070   Code   RO          116    i.pps_update_handle  p6a_demo.o
    0x00017ce4   0x00017ce4   0x000002e4   Code   RO          742    i.rxbr_irq1_callback  CVWL668T.lib(hal_internal_vsync.o)
    0x00017fc8   0x00017fc8   0x0000003a   Code   RO          117    i.send_panel_init_code  p6a_demo.o
    0x00018002   0x00018002   0x00000002   PAD
    0x00018004   0x00018004   0x00000044   Code   RO          743    i.soft_double_buffer_update  CVWL668T.lib(hal_internal_vsync.o)
    0x00018048   0x00018048   0x0000006c   Code   RO          744    i.soft_gen_te       CVWL668T.lib(hal_internal_vsync.o)
    0x000180b4   0x000180b4   0x000000e0   Code   RO          745    i.soft_gen_te_double_buffer  CVWL668T.lib(hal_internal_vsync.o)
    0x00018194   0x00018194   0x00000038   Code   RO          746    i.soft_pro_motion_init  CVWL668T.lib(hal_internal_vsync.o)
    0x000181cc   0x000181cc   0x00000038   Code   RO          118    i.soft_swire_init   p6a_demo.o
    0x00018204   0x00018204   0x0000002e   Code   RO          119    i.soft_swire_start  p6a_demo.o
    0x00018232   0x00018232   0x00000002   PAD
    0x00018234   0x00018234   0x00000048   Code   RO          120    i.soft_swire_timer_callback  p6a_demo.o
    0x0001827c   0x0001827c   0x00000024   Code   RO          747    i.soft_tear_adjust_line  CVWL668T.lib(hal_internal_vsync.o)
    0x000182a0   0x000182a0   0x000000ac   Code   RO          852    i.svs_direct_mode_setting  CVWL668T.lib(hal_internal_svs.o)
    0x0001834c   0x0001834c   0x0000001c   Code   RO          853    i.svs_get_rel_intv  CVWL668T.lib(hal_internal_svs.o)
    0x00018368   0x00018368   0x000000b0   Code   RO          854    i.svs_sync_handle   CVWL668T.lib(hal_internal_svs.o)
    0x00018418   0x00018418   0x000000cc   Code   RO          855    i.svs_wait_fr_stab  CVWL668T.lib(hal_internal_svs.o)
    0x000184e4   0x000184e4   0x0000010c   Code   RO          856    i.svs_wait_start    CVWL668T.lib(hal_internal_svs.o)
    0x000185f0   0x000185f0   0x00000034   Code   RO          674    i.tau_log_init      CVWL668T.lib(tau_log.o)
    0x00018624   0x00018624   0x00000084   Code   RO          675    i.tau_log_printf    CVWL668T.lib(tau_log.o)
    0x000186a8   0x000186a8   0x00000076   Code   RO          676    i.tau_log_push_log  CVWL668T.lib(tau_log.o)
    0x0001871e   0x0001871e   0x00000002   PAD
    0x00018720   0x00018720   0x000000b4   Code   RO          748    i.vidc_callback     CVWL668T.lib(hal_internal_vsync.o)
    0x000187d4   0x000187d4   0x00000118   Code   RO          749    i.vpre_err_reset    CVWL668T.lib(hal_internal_vsync.o)
    0x000188ec   0x000188ec   0x000010ac   Data   RO          123    .constdata          p6a_demo.o
    0x00019998   0x00019998   0x00000028   Data   RO          382    .constdata          CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x000199c0   0x000199c0   0x0000001c   Data   RO          483    .constdata          CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x000199dc   0x000199dc   0x000000b6   Data   RO          556    .constdata          CVWL668T.lib(hal_gpio.o)
    0x00019a92   0x00019a92   0x00000002   PAD
    0x00019a94   0x00019a94   0x00000030   Data   RO          702    .constdata          CVWL668T.lib(hal_uart.o)
    0x00019ac4   0x00019ac4   0x00000010   Data   RO         1780    .constdata          CVWL668T.lib(drv_uart.o)
    0x00019ad4   0x00019ad4   0x00000042   Data   RO          383    .conststring        CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00019b16   0x00019b16   0x00000002   PAD
    0x00019b18   0x00019b18   0x00000090   Data   RO          751    .conststring        CVWL668T.lib(hal_internal_vsync.o)
    0x00019ba8   0x00019ba8   0x00000046   Data   RO          800    .conststring        CVWL668T.lib(hal_internal_dcs.o)
    0x00019bee   0x00019bee   0x00000002   PAD
    0x00019bf0   0x00019bf0   0x00000020   Data   RO         2194    Region$$Table       anon$$obj.o


    Execution Region RW_IRAM1 (Exec base: 0x00070000, Load base: 0x00019c10, Size: 0x00003100, Max: 0x00008000, ABSOLUTE, COMPRESSED[0x0000014c])

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00070000   COMPRESSED   0x000000a1   Data   RW          124    .data               p6a_demo.o
    0x000700a1   COMPRESSED   0x00000003   PAD
    0x000700a4   COMPRESSED   0x00000030   Data   RW          384    .data               CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x000700d4   COMPRESSED   0x0000005c   Data   RW          484    .data               CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00070130   COMPRESSED   0x00000001   Data   RW          679    .data               CVWL668T.lib(tau_log.o)
    0x00070131   COMPRESSED   0x00000003   PAD
    0x00070134   COMPRESSED   0x00000018   Data   RW          703    .data               CVWL668T.lib(hal_uart.o)
    0x0007014c   COMPRESSED   0x00000010   Data   RW          752    .data               CVWL668T.lib(hal_internal_vsync.o)
    0x0007015c   COMPRESSED   0x00000024   Data   RW          801    .data               CVWL668T.lib(hal_internal_dcs.o)
    0x00070180   COMPRESSED   0x0000000c   Data   RW          885    .data               CVWL668T.lib(drv_common.o)
    0x0007018c   COMPRESSED   0x00000001   Data   RW          886    .data               CVWL668T.lib(drv_common.o)
    0x0007018d   COMPRESSED   0x00000003   PAD
    0x00070190   COMPRESSED   0x00000004   Data   RW          972    .data               CVWL668T.lib(drv_gpio.o)
    0x00070194   COMPRESSED   0x00000050   Data   RW         1149    .data               CVWL668T.lib(drv_timer.o)
    0x000701e4   COMPRESSED   0x00000004   Data   RW         1190    .data               CVWL668T.lib(drv_se.o)
    0x000701e8   COMPRESSED   0x00000001   Data   RW         1230    .data               CVWL668T.lib(drv_dsi_rx.o)
    0x000701e9   COMPRESSED   0x00000003   PAD
    0x000701ec   COMPRESSED   0x00000008   Data   RW         1565    .data               CVWL668T.lib(drv_rxbr.o)
    0x000701f4   COMPRESSED   0x00000004   Data   RW         1652    .data               CVWL668T.lib(drv_vidc.o)
    0x000701f8   COMPRESSED   0x00000190   Data   RW         1727    .data               CVWL668T.lib(drv_dma.o)
    0x00070388   COMPRESSED   0x00000004   Data   RW         2170    .data               mc_p.l(stdout.o)
    0x0007038c        -       0x000000d0   Zero   RW          381    .bss                CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x0007045c        -       0x000000b8   Zero   RW          482    .bss                CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00070514        -       0x00000100   Zero   RW          678    .bss                CVWL668T.lib(tau_log.o)
    0x00070614        -       0x00000044   Zero   RW          750    .bss                CVWL668T.lib(hal_internal_vsync.o)
    0x00070658        -       0x00000800   Zero   RW          798    .bss                CVWL668T.lib(hal_internal_dcs.o)
    0x00070e58        -       0x000000ff   Zero   RW          799    .bss                CVWL668T.lib(hal_internal_dcs.o)
    0x00070f57   COMPRESSED   0x00000001   PAD
    0x00070f58        -       0x00000044   Zero   RW          827    .bss                CVWL668T.lib(hal_internal_fb.o)
    0x00070f9c        -       0x00000044   Zero   RW          857    .bss                CVWL668T.lib(hal_internal_svs.o)
    0x00070fe0        -       0x00000040   Zero   RW          971    .bss                CVWL668T.lib(drv_gpio.o)
    0x00071020        -       0x0000106c   Zero   RW         1173    .bss                CVWL668T.lib(dcs_packet_fifo.o)
    0x0007208c        -       0x00000010   Zero   RW         1725    .bss                CVWL668T.lib(drv_dma.o)
    0x0007209c        -       0x00000060   Zero   RW         1779    .bss                CVWL668T.lib(drv_uart.o)
    0x000720fc   COMPRESSED   0x00000004   PAD
    0x00072100        -       0x00001000   Zero   RW          331    STACK               startup_armcm0.o


==============================================================================

Image component sizes


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Object Name

        24          4          0          0          0        585   board.o
        64         32          0          0          0      10487   main.o
      2040        406       4268        161          0      26964   p6a_demo.o
       120         18        192          0       4096       2172   startup_armcm0.o

    ----------------------------------------------------------------------
      2256        460       4492        164       4096      40208   Object Totals
         0          0         32          0          0          0   (incl. Generated)
         8          0          0          3          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Member Name

       216         32          0          0       4204        252   dcs_packet_fifo.o
       104         62         28         13          0        192   drv_common.o
       504         80          0          0          0        672   drv_crgu.o
       136         22          0        400         16        196   drv_dma.o
       116         26          0          0          0        188   drv_dsc_dec.o
      1880        672          0          1          0       1280   drv_dsi_rx.o
      1704        306          0          0          0       2036   drv_dsi_tx.o
       148          0          0          0          0        260   drv_efuse.o
       196         22          0          4         64        808   drv_gpio.o
      1064        162          0          0          0       1560   drv_lcdc.o
       658        104          0          0          0       1240   drv_memc.o
        40          0          0          0          0        120   drv_phy_common.o
       188         60          0          0          0        308   drv_pwr.o
       514        102          0          8          0       1120   drv_rxbr.o
       972        266          0          4          0        488   drv_se.o
        88         18          0          0          0        188   drv_sys_cfg.o
       386         44          0         80          0        876   drv_timer.o
      1172         54         16          0         96        980   drv_uart.o
       824        152          0          4          0       1700   drv_vidc.o
      2570        182        106         48        208       1120   hal_dsi_rx_ctrl.o
      4158        320         50         92        184       2076   hal_dsi_tx_ctrl.o
       244         10        182          0          0        404   hal_gpio.o
      2140        506         70         36       2303        652   hal_internal_dcs.o
      1348         58          0          0         68        700   hal_internal_fb.o
      1172        182          0          0         68        840   hal_internal_svs.o
      3812        798        144         16         68       1628   hal_internal_vsync.o
        16          0          0          0          0        136   hal_pwr.o
       308         56          0          0          0        136   hal_system.o
       164          0          0          0          0        276   hal_timer.o
       176         18         48         24          0        144   hal_uart.o
        68          4          0          0          0        136   tau_delay.o
       354         30         16          1        256        320   tau_log.o
       200         20          0          0          0         76   ceil.o
        86          0          0          0          0          0   __dczerorl2.o
         0          0          0          0          0          0   entry.o
         0          0          0          0          0          0   entry10a.o
         0          0          0          0          0          0   entry11a.o
         8          4          0          0          0          0   entry2.o
         4          0          0          0          0          0   entry5.o
         0          0          0          0          0          0   entry7b.o
         0          0          0          0          0          0   entry8b.o
         8          4          0          0          0          0   entry9a.o
        30          0          0          0          0          0   handlers.o
        40          0          0          0          0         72   idiv.o
        36          8          0          0          0         68   init.o
         0          0          0          0          0          0   iusefp.o
        32          0          0          0          0         68   llshl.o
        38          0          0          0          0         68   llsshr.o
        34          0          0          0          0         68   llushr.o
        26          0          0          0          0         72   memcmp.o
        36          0          0          0          0         60   memcpya.o
        36          0          0          0          0        100   memseta.o
      2298        104          0          0          0        544   printfa.o
         0          0          0          4          0          0   stdout.o
        14          0          0          0          0         60   strlen.o
        44          0          0          0          0         72   uidiv.o
        96          0          0          0          0         84   uldiv.o
        40          2          0          0          0         68   cdrcmple.o
        20          0          0          0          0         68   cfcmple.o
        20          0          0          0          0         68   cfrcmple.o
        56          0          0          0          0         68   d2f.o
       356          4          0          0          0        140   dadd.o
       240          6          0          0          0         84   ddiv.o
       236          0          0          0          0        216   depilogue.o
        60         10          0          0          0         68   dfixui.o
        64         10          0          0          0         68   dfixul.o
        28          4          0          0          0         68   dfltui.o
       208          6          0          0          0         88   dmul.o
        40          0          0          0          0         60   f2d.o
       178          0          0          0          0        108   fadd.o
       124          0          0          0          0         72   fdiv.o
       130          0          0          0          0        144   fepilogue.o
        40          0          0          0          0         60   ffixui.o
        14          0          0          0          0         68   ffltui.o
       122          0          0          0          0         72   fmul.o
        24          0          0          0          0         60   fscalb.o

    ----------------------------------------------------------------------
     32536       4530        668        744       7540      26092   Library Totals
        30          0          8          9          5          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Name

     27440       4348        660        731       7535      23032   CVWL668T.lib
       200         20          0          0          0         76   m_ps.l
      2866        120          0          4          0       1336   mc_p.l
      2000         42          0          0          0       1648   mf_p.l

    ----------------------------------------------------------------------
     32536       4530        668        744       7540      26092   Library Totals

    ----------------------------------------------------------------------

==============================================================================


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   

     34792       4990       5160        908      11636      49032   Grand Totals
     34792       4990       5160        332      11636      49032   ELF Image Totals (compressed)
     34792       4990       5160        332          0          0   ROM Totals

==============================================================================

    Total RO  Size (Code + RO Data)                39952 (  39.02kB)
    Total RW  Size (RW Data + ZI Data)             12544 (  12.25kB)
    Total ROM Size (Code + RO Data + RW Data)      40284 (  39.34kB)

==============================================================================

