Component: ARM Compiler 5.06 update 6 (build 750) Tool: armlink [4d35ed]

==============================================================================

Section Cross References

    main.o(i.main) refers to board.o(i.board_Init) for board_Init
    main.o(i.main) refers to p6a_demo.o(i.google_p6a_demo) for google_p6a_demo
    main.o(i.main) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.Gpio_swire_output) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    p6a_demo.o(i.Gpio_swire_output) refers to tau_delay.o(i.delayMs) for delayMs
    p6a_demo.o(i.Gpio_swire_output) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    p6a_demo.o(i.Gpio_swire_output) refers to tau_delay.o(i.delayUs) for delayUs
    p6a_demo.o(i.Panel_CCM) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) for hal_dsi_tx_ctrl_set_ccm
    p6a_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) for hal_dsi_rx_ctrl_send_ack_cmd
    p6a_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) for hal_dsi_rx_ctrl_get_max_ret_size
    p6a_demo.o(i.ap_dcs_read) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.ap_dcs_read) refers to p6a_demo.o(.data) for g_rx_ctrl_handle
    p6a_demo.o(i.ap_dcs_set_backlight) refers to idiv.o(.text) for __aeabi_idivmod
    p6a_demo.o(i.ap_dcs_set_backlight) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    p6a_demo.o(i.ap_dcs_set_backlight) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.ap_dcs_set_backlight) refers to p6a_demo.o(.data) for rd_51_val
    p6a_demo.o(i.ap_dcs_set_display_off) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.ap_dcs_set_display_off) refers to p6a_demo.o(.data) for panel_display_done
    p6a_demo.o(i.ap_dcs_set_display_on) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    p6a_demo.o(i.ap_dcs_set_display_on) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to tau_delay.o(i.delayMs) for delayMs
    p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to hal_swire.o(i.hal_swire_enable) for hal_swire_enable
    p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to p6a_demo.o(i.ap_rstn_pull_down_cb) for ap_rstn_pull_down_cb
    p6a_demo.o(i.ap_dcs_set_exit_idle_mode) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) for hal_dsi_rx_ctrl_set_hw_cmd_filter
    p6a_demo.o(i.ap_dcs_set_exit_idle_mode) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.ap_dcs_set_exit_idle_mode) refers to p6a_demo.o(.data) for sg_exit_idle_mode_flag
    p6a_demo.o(i.ap_dcs_set_exit_sleep_mode) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.ap_dcs_set_frame_change) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode) for hal_dsi_tx_ctrl_set_tear_mode
    p6a_demo.o(i.ap_dcs_set_frame_change) refers to p6a_demo.o(.data) for g_tx_ctrl_handle
    p6a_demo.o(i.ap_rstn_pull_down_cb) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.ap_rstn_pull_down_cb) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    p6a_demo.o(i.ap_rstn_pull_down_cb) refers to p6a_demo.o(.data) for sg_system_suspend
    p6a_demo.o(i.ap_rstn_pull_high_cb) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    p6a_demo.o(i.ap_rstn_pull_high_cb) refers to p6a_demo.o(.data) for sg_system_resume
    p6a_demo.o(i.ap_set_FPS_B1) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    p6a_demo.o(i.app_display_init) refers to p6a_demo.o(i.app_mipi_rx_init) for app_mipi_rx_init
    p6a_demo.o(i.app_display_init) refers to hal_pwr.o(i.hal_pwr_get_vcc_power_ready) for hal_pwr_get_vcc_power_ready
    p6a_demo.o(i.app_display_init) refers to p6a_demo.o(i.app_gpio_init) for app_gpio_init
    p6a_demo.o(i.app_display_init) refers to hal_swire.o(i.hal_swire_init) for hal_swire_init
    p6a_demo.o(i.app_display_init) refers to hal_swire.o(i.hal_swire_set_timer) for hal_swire_set_timer
    p6a_demo.o(i.app_display_init) refers to p6a_demo.o(i.app_mipi_tx_init) for app_mipi_tx_init
    p6a_demo.o(i.app_display_init) refers to p6a_demo.o(i.app_mipi_tx_start) for app_mipi_tx_start
    p6a_demo.o(i.app_gpio_init) refers to hal_gpio.o(i.hal_gpio_config_pad) for hal_gpio_config_pad
    p6a_demo.o(i.app_gpio_init) refers to p6a_demo.o(.constdata) for .constdata
    p6a_demo.o(i.app_init_panel) refers to p6a_demo.o(i.app_tx_panel_reset) for app_tx_panel_reset
    p6a_demo.o(i.app_init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    p6a_demo.o(i.app_init_panel) refers to tau_delay.o(i.delayMs) for delayMs
    p6a_demo.o(i.app_init_panel) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    p6a_demo.o(i.app_init_panel) refers to hal_swire.o(i.hal_swire_enable) for hal_swire_enable
    p6a_demo.o(i.app_init_panel) refers to hal_swire.o(i.hal_swire_set_pulse) for hal_swire_set_pulse
    p6a_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) for hal_dsi_rx_ctrl_create_handle
    p6a_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) for hal_dsi_rx_ctrl_pre_init_pps
    p6a_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    p6a_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    p6a_demo.o(i.app_mipi_rx_init) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.app_mipi_rx_init) refers to p6a_demo.o(.data) for g_rx_ctrl_handle
    p6a_demo.o(i.app_mipi_rx_init) refers to p6a_demo.o(.constdata) for g_cus_rx_dcs_execute_table
    p6a_demo.o(i.app_mipi_rx_init) refers to p6a_demo.o(i.ap_dcs_read) for ap_dcs_read
    p6a_demo.o(i.app_mipi_rx_init) refers to p6a_demo.o(i.pps_update_handle) for pps_update_handle
    p6a_demo.o(i.app_mipi_tx_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) for hal_dsi_tx_ctrl_create_handle
    p6a_demo.o(i.app_mipi_tx_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    p6a_demo.o(i.app_mipi_tx_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) for hal_dsi_tx_ctrl_set_overwrite_rgb
    p6a_demo.o(i.app_mipi_tx_init) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.app_mipi_tx_init) refers to p6a_demo.o(.data) for g_tx_ctrl_handle
    p6a_demo.o(i.app_mipi_tx_start) refers to p6a_demo.o(i.app_init_panel) for app_init_panel
    p6a_demo.o(i.app_mipi_tx_start) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    p6a_demo.o(i.app_mipi_tx_start) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode) for hal_dsi_tx_ctrl_set_tear_mode
    p6a_demo.o(i.app_mipi_tx_start) refers to hal_swire.o(i.hal_swire_set_pulse) for hal_swire_set_pulse
    p6a_demo.o(i.app_mipi_tx_start) refers to tau_delay.o(i.delayMs) for delayMs
    p6a_demo.o(i.app_mipi_tx_start) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    p6a_demo.o(i.app_mipi_tx_start) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.app_mipi_tx_start) refers to p6a_demo.o(.data) for g_tx_ctrl_handle
    p6a_demo.o(i.app_system_process) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.app_system_process) refers to p6a_demo.o(i.app_system_suspend) for app_system_suspend
    p6a_demo.o(i.app_system_process) refers to p6a_demo.o(i.app_system_resume) for app_system_resume
    p6a_demo.o(i.app_system_process) refers to p6a_demo.o(.data) for sg_system_suspend
    p6a_demo.o(i.app_system_resume) refers to hal_pwr.o(i.hal_pwr_exit_sleep_mode) for hal_pwr_exit_sleep_mode
    p6a_demo.o(i.app_system_resume) refers to p6a_demo.o(i.app_display_init) for app_display_init
    p6a_demo.o(i.app_system_resume) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.app_system_suspend) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) for hal_dsi_tx_ctrl_stop
    p6a_demo.o(i.app_system_suspend) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) for hal_dsi_tx_ctrl_deinit
    p6a_demo.o(i.app_system_suspend) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) for hal_dsi_rx_ctrl_stop
    p6a_demo.o(i.app_system_suspend) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) for hal_dsi_rx_ctrl_deinit
    p6a_demo.o(i.app_system_suspend) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    p6a_demo.o(i.app_system_suspend) refers to hal_swire.o(i.hal_swire_deinit) for hal_swire_deinit
    p6a_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_set_sleep_mode_power) for hal_pwr_set_sleep_mode_power
    p6a_demo.o(i.app_system_suspend) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    p6a_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_enter_normal_sleep_mode) for hal_pwr_enter_normal_sleep_mode
    p6a_demo.o(i.app_system_suspend) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) for hal_pwr_set_stop_sleep_wakeup_pin
    p6a_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) for hal_pwr_enter_stop_sleep_mode
    p6a_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode) for hal_pwr_enter_deep_sleep_mode
    p6a_demo.o(i.app_system_suspend) refers to p6a_demo.o(.data) for g_tx_ctrl_handle
    p6a_demo.o(i.app_system_suspend) refers to p6a_demo.o(i.ap_rstn_pull_high_cb) for ap_rstn_pull_high_cb
    p6a_demo.o(i.app_tx_panel_reset) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    p6a_demo.o(i.app_tx_panel_reset) refers to tau_delay.o(i.delayMs) for delayMs
    p6a_demo.o(i.google_p6a_demo) refers to hal_pwr.o(i.hal_pwr_set_main_power) for hal_pwr_set_main_power
    p6a_demo.o(i.google_p6a_demo) refers to p6a_demo.o(i.app_display_init) for app_display_init
    p6a_demo.o(i.google_p6a_demo) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    p6a_demo.o(i.google_p6a_demo) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) for hal_dsi_rx_ctrl_dcs_async_handler
    p6a_demo.o(i.google_p6a_demo) refers to p6a_demo.o(i.app_system_process) for app_system_process
    p6a_demo.o(i.google_p6a_demo) refers to p6a_demo.o(.data) for g_rx_ctrl_handle
    p6a_demo.o(i.pps_update_handle) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode) for hal_dsi_tx_ctrl_set_tear_mode
    p6a_demo.o(i.pps_update_handle) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) for hal_dsi_rx_ctrl_toggle_resolution
    p6a_demo.o(i.pps_update_handle) refers to p6a_demo.o(.data) for g_rx_ctrl_handle
    p6a_demo.o(i.soft_te_timer_cb) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) for hal_dsi_tx_ctrl_gen_a_tear_signal
    p6a_demo.o(i.soft_te_timer_cb) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    p6a_demo.o(i.soft_te_timer_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode) for hal_dsi_tx_ctrl_set_tear_mode
    p6a_demo.o(i.soft_te_timer_init) refers to hal_timer.o(i.hal_timer_init) for hal_timer_init
    p6a_demo.o(i.soft_te_timer_init) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    p6a_demo.o(i.soft_te_timer_init) refers to p6a_demo.o(.data) for g_tx_ctrl_handle
    p6a_demo.o(i.soft_te_timer_init) refers to p6a_demo.o(i.soft_te_timer_cb) for soft_te_timer_cb
    p6a_demo.o(.constdata) refers to p6a_demo.o(i.ap_dcs_set_display_on) for ap_dcs_set_display_on
    p6a_demo.o(.constdata) refers to p6a_demo.o(i.ap_dcs_set_display_off) for ap_dcs_set_display_off
    p6a_demo.o(.constdata) refers to p6a_demo.o(i.ap_dcs_set_backlight) for ap_dcs_set_backlight
    p6a_demo.o(.constdata) refers to p6a_demo.o(i.ap_dcs_set_enter_sleep_mode) for ap_dcs_set_enter_sleep_mode
    p6a_demo.o(.constdata) refers to p6a_demo.o(i.ap_dcs_set_exit_sleep_mode) for ap_dcs_set_exit_sleep_mode
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_init) for hal_system_init
    board.o(i.board_Init) refers to tau_log.o(i.tau_log_init) for tau_log_init
    startup_armcm0.o(RESET) refers to startup_armcm0.o(STACK) for __initial_sp
    startup_armcm0.o(RESET) refers to startup_armcm0.o(.text) for Reset_Handler
    startup_armcm0.o(RESET) refers to drv_common.o(i.HardFault_Handler) for HardFault_Handler
    startup_armcm0.o(RESET) refers to drv_common.o(i.SysTick_Handler) for SysTick_Handler
    startup_armcm0.o(RESET) refers to drv_vidc.o(i.VIDC_IRQn_Handler) for VIDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to hal_internal_vsync.o(i.LCDC_IRQn_Handler) for LCDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) for MIPI_RX_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler) for MIPI_TX_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_memc.o(i.MEMC_IRQn_Handler) for MEMC_IRQn_Handler
    startup_armcm0.o(RESET) refers to hal_internal_dcs.o(i.VPRE_IRQn_Handler) for VPRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_dma.o(i.DMA_IRQn_Handler) for DMA_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER0_IRQn_Handler) for TIMER0_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER1_IRQn_Handler) for TIMER1_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER2_IRQn_Handler) for TIMER2_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER3_IRQn_Handler) for TIMER3_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_uart.o(i.UART_IRQn_Handler) for UART_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_rxbr.o(i.VPRE1_IRQn_Handler) for VPRE1_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_swire.o(i.SWIRE_IRQn_Handler) for SWIRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.AP_NRESET_IRQn_Handler) for AP_NRESET_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT0_IRQn_Handler) for EXTI_INT0_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT1_IRQn_Handler) for EXTI_INT1_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT2_IRQn_Handler) for EXTI_INT2_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT3_IRQn_Handler) for EXTI_INT3_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT4_IRQn_Handler) for EXTI_INT4_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT5_IRQn_Handler) for EXTI_INT5_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT6_IRQn_Handler) for EXTI_INT6_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT7_IRQn_Handler) for EXTI_INT7_IRQn_Handler
    startup_armcm0.o(.text) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd) refers to drv_rxbr.o(i.drv_rxbr_set_ack_pkt_md) for drv_rxbr_set_ack_pkt_md
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_lpdt_fifo_status) for drv_dsi_rx_get_lpdt_fifo_status
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) for dcs_packet_get_fifo_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) for dcs_packet_free_fifo_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) for hal_internal_vsync_get_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_reset_modules) for drv_crgu_reset_modules
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_line) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_line) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_line) refers to hal_dsi_rx_ctrl.o(i.swap_uint16_t) for swap_uint16_t
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_line) refers to fflti.o(.text) for __aeabi_i2f
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_line) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_line) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data_ex) for hal_dsi_rx_ctrl_set_pixel_data_ex
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_rxbr.o(i.drv_rxbr_swpxl_clr) for drv_rxbr_swpxl_clr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_rxbr.o(i.drv_rxbr_set_cmd_filter) for drv_rxbr_set_cmd_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_vidc.o(i.drv_vidc_set_src_parameter) for drv_vidc_set_src_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_vidc.o(i.drv_vidc_set_pu_ctrl) for drv_vidc_set_pu_ctrl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_rxbr.o(i.drv_rxbr_set_swpxl_data) for drv_rxbr_set_swpxl_data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg) for drv_dsi_rx_set_ddi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) for hal_dsi_rx_ctrl_set_rx_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg) for drv_dsi_rx_set_ipi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.constdata) for .constdata
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_force_video_crtl) refers to drv_dsi_rx.o(i.drv_dsi_rx_force_video_crtl) for drv_dsi_rx_force_video_crtl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_cap_pixel_color) refers to drv_vidc.o(i.drv_vidc_get_status2) for drv_vidc_get_status2
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size) for drv_dsi_rx_get_max_ret_size
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) for hal_dsi_rx_ctrl_init_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_rx) for hal_internal_vsync_init_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) for hal_dsi_rx_ctrl_init_dsi_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) for hal_dsi_rx_ctrl_init_rxbr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_irqen) for drv_dsc_dec_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) for hal_dsi_rx_ctrl_init_vidc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) for hal_dsi_rx_ctrl_init_memc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_se.o(i.drv_se_start_rx) for drv_se_start_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_pwr.o(i.drv_pwr_set_pll_clk) for drv_pwr_set_pll_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_clk) for drv_crgu_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dsc_clk) for drv_crgu_set_dsc_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_vidc_clk) for drv_crgu_set_vidc_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_fb_clk) for drv_crgu_set_fb_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg) for drv_dsi_rx_set_ctrl_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) for drv_dsi_rx_set_up_phy
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap) for drv_dsi_rx_set_lane_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_crc_en) for drv_dsi_rx_set_ddi_crc_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_ycbcr_frmt) for drv_dsi_rx_set_ipi_ycbcr_frmt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_tear_resp_en) for drv_dsi_rx_set_tear_resp_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_inten) for drv_dsi_rx_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc) for drv_dsi_rx_set_check_crc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt) for drv_dsi_rx_set_resp_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_mode) for drv_memc_set_ltpo_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_fs_en_conditions) for drv_memc_set_fs_en_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_lcdc_st_conditions) for drv_memc_set_lcdc_st_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_vidc_sync_cnt) for drv_memc_set_vidc_sync_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_double_buffer) for drv_memc_set_double_buffer
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_circ_mode_enable) for drv_memc_set_circ_mode_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_active_height) for drv_memc_set_active_height
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_pu_thres) for drv_memc_set_ltpo_pu_thres
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_color_format) for drv_rxbr_set_color_format
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th) for drv_rxbr_set_ltpo_drop_th
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_cfg) for drv_rxbr_set_usr_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_col) for drv_rxbr_set_usr_col
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_row) for drv_rxbr_set_usr_row
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg) for drv_rxbr_hline_rcv_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) for hal_intl_dcs_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_src_parameter) for drv_vidc_set_src_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pentile_swap) for drv_vidc_set_pentile_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_dst_parameter) for drv_vidc_set_dst_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_circ_mode_enable) for drv_vidc_set_circ_mode_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_init_module_enable) for drv_vidc_init_module_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_dither_config) for drv_vidc_set_dither_config
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_vintp_config) for drv_vidc_set_vintp_config
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_rotation) for drv_vidc_set_rotation
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef0) for drv_vidc_set_scld_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef1) for drv_vidc_set_scld_hcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef0) for drv_vidc_set_scld_vcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef1) for drv_vidc_set_scld_vcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_honly_hinitr) for drv_vidc_set_honly_hinitr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_honly_hinitb) for drv_vidc_set_honly_hinitb
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_honly_hcoef0) for drv_vidc_set_honly_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_mirror) for drv_vidc_set_mirror
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pu_ctrl) for drv_vidc_set_pu_ctrl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_dsi_rx_ctrl.o(.constdata) for .constdata
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to hal_internal_vsync.o(i.hal_internal_sync_register_rx_callback) for hal_internal_sync_register_rx_callback
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to drv_vidc.o(i.drv_vidc_set_irq_line) for drv_vidc_set_irq_line
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_write_cmd_entry) refers to hal_internal_dcs.o(i.hal_intl_dcs_register_write_cmd_entry) for hal_intl_dcs_register_write_cmd_entry
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header) for drv_rxbr_set_ack_pkt_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack) refers to drv_rxbr.o(i.drv_rxbr_set_cmd_response) for drv_rxbr_set_cmd_response
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) for hal_intl_dcs_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cap_pixel_pos) refers to drv_vidc.o(i.drv_vidc_debug_cap_pixel) for drv_vidc_debug_cap_pixel
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_check_crc) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc) for drv_dsi_rx_set_check_crc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_check_crc) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) for drv_dsi_rx_calc_ipi_tx_delay
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg) for drv_dsi_rx_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_log_level) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_drv_log_level) for drv_dsi_rx_set_drv_log_level
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to drv_rxbr.o(i.drv_rxbr_sw_reset) for drv_rxbr_sw_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data_ex) refers to drv_rxbr.o(i.drv_rxbr_sw_reset) for drv_rxbr_sw_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data_ex) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) for hal_dsi_rx_ctrl_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) for hal_intl_svs_update_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_clk) for drv_crgu_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_dsi_rx.o(i.drv_dsi_rx_power_up) for drv_dsi_rx_power_up
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) for hal_internal_vsync_toggle_input_frame_rate
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) for hal_internal_sync_input_resolution_change
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) for hal_dsi_tx_ctrl_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg) for drv_dsi_tx_phy_time_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) for drv_dsi_tx_phy_test_setup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready) for drv_dsi_tx_phy_status_ready
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_crgu.o(i.drv_crgu_reset_modules) for drv_crgu_reset_modules
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_reset_modules) for drv_crgu_reset_modules
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb) for hal_internal_sync_register_lcdc_cb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) for hal_internal_sync_set_fb_setting_manual
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) for hal_lcdc_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_frame) refers to drv_lcdc.o(i.drv_lcdc_fixed_frame_output) for drv_lcdc_fixed_frame_output
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_get_tear_mode) for drv_memc_get_tear_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_gen_a_tear_signal) for drv_memc_gen_a_tear_signal
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_tx) for hal_internal_vsync_init_tx
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb) for hal_internal_sync_register_lcdc_cb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) for hal_dsi_tx_ctrl_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) for hal_dsi_tx_init_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) for hal_dsi_tx_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) for hal_lcdc_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) for hal_lcdc_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready) for drv_dsi_tx_phy_status_ready
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) for hal_nonshadow_func_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_vsync_func_update) for hal_vsync_func_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_overwrite_enable) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_overwrite_enable) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_partial_disp_enable) refers to drv_lcdc.o(i.drv_lcdc_part_display_config) for drv_lcdc_part_display_config
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_partial_disp_enable) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload) for drv_dsi_tx_command_get_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) for hal_nonshadow_func_req_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_sync_line) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) for hal_internal_vsync_set_sync_line
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_sync_line) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) for hal_nonshadow_func_req_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) for hal_nonshadow_func_req_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) for hal_nonshadow_func_req_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb) for drv_lcdc_config_overwrite_rgb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_vpg) for drv_dsi_tx_set_vpg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) for hal_dsi_tx_ctrl_draw_flick
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp) for drv_dsi_tx_phy_clock_lane_auto_lp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_cfg_int_frame) for drv_lcdc_cfg_int_frame
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_enable_shadow_reg) for drv_lcdc_enable_shadow_reg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_start) for hal_lcdc_start
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_lcdc.o(i.drv_lcdc_stop_display) for drv_lcdc_stop_display
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) for hal_dsi_tx_ctrl_read_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg) for drv_dsi_tx_video_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack) for drv_dsi_tx_set_bta_ack
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time) for drv_dsi_tx_dpi_lpcmd_time
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode) for drv_dsi_tx_phy_lane_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode) for drv_dsi_tx_dpi_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity) for drv_dsi_tx_dpi_polarity
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_response_mode) for drv_dsi_tx_response_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div) for drv_dsi_tx_set_time_out_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg) for drv_dsi_tx_timeout_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp) for drv_dsi_tx_phy_clock_lane_auto_lp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_int) for drv_dsi_tx_config_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to drv_crgu.o(i.drv_crgu_set_dpi_clk) for drv_crgu_set_dpi_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to hal_dsi_tx_ctrl.o(.constdata) for .constdata
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg) for drv_dsi_tx_phy_time_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) for drv_dsi_tx_phy_test_setup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update) for hal_dsi_tx_timing_info_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) for hal_dsi_tx_cmd_mode_cal_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size) for drv_dsi_tx_edpi_cmd_size
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) for hal_dsi_tx_init_phy_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) for hal_dsi_tx_init_dpi_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) for hal_dsi_tx_vid_mode_cal_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing) for hal_dsi_tx_init_vid_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk) for drv_dsi_tx_set_video_chunk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing) for drv_dsi_tx_set_video_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_header) for drv_dsi_tx_command_header
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update) refers to d2f.o(.text) for __aeabi_d2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_internal_svs.o(i.hal_intl_svs_init_tx) for hal_intl_svs_init_tx
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) for hal_tx_frame_rate_adjust
    hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) refers to drv_lcdc.o(i.drv_lcdc_endianness_config) for drv_lcdc_endianness_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) refers to drv_lcdc.o(i.drv_lcdc_crop_hact) for drv_lcdc_crop_hact
    hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) for hal_lcdc_postproc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) for hal_lcdc_displayproc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) for hal_intl_fb_get_tx_fb_info
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) for hal_lcdc_timinggen_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to drv_lcdc.o(i.drv_lcdc_config_int) for drv_lcdc_config_int
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fscalb.o(.text) for __ARM_scalbnf
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_lcdc_clk) for drv_crgu_set_lcdc_clk
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) for hal_intl_fb_get_tx_fb_info
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) for hal_lcdc_upscaler_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_fldc_config) for drv_lcdc_fldc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_bcsa_config) for drv_lcdc_bcsa_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_fc_config) for drv_lcdc_fc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_edge_dect_config) for drv_lcdc_edge_dect_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_edge_enh_config) for drv_lcdc_edge_enh_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_vintp_mode_config) for drv_lcdc_vintp_mode_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_dith_config) for drv_lcdc_dith_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to drv_lcdc.o(i.drv_lcdc_vid_hw_start) for drv_lcdc_vid_hw_start
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to drv_lcdc.o(i.drv_lcdc_cmd_start) for drv_lcdc_cmd_start
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to drv_lcdc.o(i.drv_lcdc_ctrl_flow) for drv_lcdc_ctrl_flow
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to drv_lcdc.o(i.drv_lcdc_config_src_parameter) for drv_lcdc_config_src_parameter
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to drv_lcdc.o(i.drv_lcdc_set_prefetch) for drv_lcdc_set_prefetch
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for sg_pq_para
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_bcsa_config) for drv_lcdc_bcsa_config
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_fc_config) for drv_lcdc_fc_config
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_edge_dect_config) for drv_lcdc_edge_dect_config
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_edge_enh_config) for drv_lcdc_edge_enh_config
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for sg_pq_para
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to cfcmple.o(.text) for __aeabi_cfcmple
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_vsync_func_update) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_vsync_func_update) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_gpio.o(i.hal_gpio_config_pad) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_config_pad) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    hal_gpio.o(i.hal_gpio_config_pad) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    hal_gpio.o(i.hal_gpio_ctrl_eint) refers to drv_gpio.o(i.drv_gpio_set_int) for drv_gpio_set_int
    hal_gpio.o(i.hal_gpio_get_input_data) refers to drv_gpio.o(i.drv_gpio_get_input_data) for drv_gpio_get_input_data
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_eint) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group) for drv_sys_cfg_sel_gpio_group
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig) for drv_sys_cfg_sel_int_trig
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_init_input) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_input) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_init_output) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_reg_eint_cb) refers to drv_gpio.o(i.drv_gpio_register_callback) for drv_gpio_register_callback
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_gpio.o(i.drv_gpio_register_ap_reset_callback) for drv_gpio_register_ap_reset_callback
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) for drv_sys_cfg_sel_ap_rst_trig
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_high_impedance) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode) for drv_gpio_set_mode
    hal_gpio.o(i.hal_gpio_set_mode) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_output_data) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to hal_gpio.o(.constdata) for .constdata
    hal_swire.o(i.hal_swire_deinit) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    hal_swire.o(i.hal_swire_deinit) refers to drv_swire.o(i.drv_swire_enable) for drv_swire_enable
    hal_swire.o(i.hal_swire_deinit) refers to drv_swire.o(i.drv_swire_register_callback) for drv_swire_register_callback
    hal_swire.o(i.hal_swire_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_swire.o(i.hal_swire_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_swire.o(i.hal_swire_deinit) refers to hal_timer.o(i.hal_timer_deinit) for hal_timer_deinit
    hal_swire.o(i.hal_swire_deinit) refers to hal_swire.o(.data) for .data
    hal_swire.o(i.hal_swire_enable) refers to drv_swire.o(i.drv_swire_set_power_down) for drv_swire_set_power_down
    hal_swire.o(i.hal_swire_enable) refers to drv_swire.o(i.drv_swire_get_pulse_count) for drv_swire_get_pulse_count
    hal_swire.o(i.hal_swire_enable) refers to drv_swire.o(i.drv_swire_set_trig_mode) for drv_swire_set_trig_mode
    hal_swire.o(i.hal_swire_enable) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_swire.o(i.hal_swire_enable) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    hal_swire.o(i.hal_swire_enable) refers to hal_swire.o(.data) for .data
    hal_swire.o(i.hal_swire_init) refers to drv_crgu.o(i.drv_crgu_set_clock_div) for drv_crgu_set_clock_div
    hal_swire.o(i.hal_swire_init) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_swire.o(i.hal_swire_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_swire.o(i.hal_swire_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_swire.o(i.hal_swire_init) refers to drv_swire.o(i.drv_swire_set_bit_time) for drv_swire_set_bit_time
    hal_swire.o(i.hal_swire_init) refers to drv_swire.o(i.drv_swire_set_power_down) for drv_swire_set_power_down
    hal_swire.o(i.hal_swire_init) refers to drv_swire.o(i.drv_swire_enable) for drv_swire_enable
    hal_swire.o(i.hal_swire_init) refers to drv_common.o(.data) for g_system_clock
    hal_swire.o(i.hal_swire_register_callback) refers to drv_swire.o(i.drv_swire_register_callback) for drv_swire_register_callback
    hal_swire.o(i.hal_swire_register_callback) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    hal_swire.o(i.hal_swire_set_pulse) refers to drv_swire.o(i.drv_swire_set_trig_mode) for drv_swire_set_trig_mode
    hal_swire.o(i.hal_swire_set_pulse) refers to drv_swire.o(i.drv_swire_set_pulse_count) for drv_swire_set_pulse_count
    hal_swire.o(i.hal_swire_set_pulse) refers to hal_swire.o(.data) for .data
    hal_swire.o(i.hal_swire_set_timer) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_swire_timer) for drv_sys_cfg_sel_swire_timer
    hal_swire.o(i.hal_swire_set_timer) refers to hal_timer.o(i.hal_timer_init) for hal_timer_init
    hal_swire.o(i.hal_swire_set_timer) refers to hal_timer.o(i.hal_timer_set_repeat) for hal_timer_set_repeat
    hal_swire.o(i.hal_swire_set_timer) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_swire.o(i.hal_swire_set_timer) refers to drv_swire.o(i.drv_swire_set_trig_mode) for drv_swire_set_trig_mode
    hal_swire.o(i.hal_swire_set_timer) refers to hal_swire.o(.data) for .data
    hal_swire.o(i.hal_swire_set_waveform) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_swire.o(i.hal_swire_set_waveform) refers to drv_swire.o(i.drv_swire_set_bit_time) for drv_swire_set_bit_time
    hal_swire.o(i.hal_swire_set_waveform) refers to drv_common.o(.data) for g_system_clock
    hal_system.o(i.hal_system_disable_systick) refers to drv_common.o(i.drv_common_disable_systick) for drv_common_disable_systick
    hal_system.o(i.hal_system_enable_systick) refers to drv_common.o(i.drv_common_enable_systick) for drv_common_enable_systick
    hal_system.o(i.hal_system_get_tick) refers to drv_common.o(i.drv_common_get_tick) for drv_common_get_tick
    hal_system.o(i.hal_system_idle_mode) refers to drv_common.o(i.drv_common_idle_mode) for drv_common_idle_mode
    hal_system.o(i.hal_system_init) refers to drv_pwr.o(i.drv_pwr_set_pll_clk) for drv_pwr_set_pll_clk
    hal_system.o(i.hal_system_init) refers to hal_system.o(i.hal_system_updata_sysclk) for hal_system_updata_sysclk
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_system.o(i.hal_system_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int) for drv_sys_cfg_clear_all_int
    hal_system.o(i.hal_system_init) refers to drv_common.o(i.drv_common_system_init) for drv_common_system_init
    hal_system.o(i.hal_system_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_system.o(i.hal_system_register_systick_cb) refers to drv_common.o(i.drv_common_systick_register_cb) for drv_common_systick_register_cb
    hal_system.o(i.hal_system_reset_chip) refers to drv_crgu.o(i.drv_crgu_reset_chip) for drv_crgu_reset_chip
    hal_system.o(i.hal_system_updata_sysclk) refers to drv_crgu.o(i.drv_crgu_set_ahb_clk) for drv_crgu_set_ahb_clk
    hal_system.o(i.hal_system_updata_sysclk) refers to drv_common.o(.data) for g_system_clock
    hal_system.o(i.hal_system_updata_sysclk) refers to drv_common.o(.data) for g_system_delay_step
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_set_repeat) for drv_timer_set_repeat
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_timer.o(i.hal_timer_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_timer.o(i.hal_timer_get_status) refers to drv_timer.o(i.drv_timer_get_status) for drv_timer_get_status
    hal_timer.o(i.hal_timer_init) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_timer.o(i.hal_timer_init) refers to drv_timer.o(i.drv_timer_set_prescaler) for drv_timer_set_prescaler
    hal_timer.o(i.hal_timer_set_repeat) refers to drv_timer.o(i.drv_timer_set_repeat) for drv_timer_set_repeat
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_pwr.o(i.hal_pwr_elvcc_close) refers to drv_pwr.o(i.drv_pwr_pwmled_electric_current) for drv_pwr_pwmled_electric_current
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_pwmled_electric_current) for drv_pwr_pwmled_electric_current
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_hv_ldo_mode_sel) for drv_pwr_hv_ldo_mode_sel
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_hv_ldo_mode_clock_sel) for drv_pwr_hv_ldo_mode_clock_sel
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_pwmled_driver_current_Big_step) for drv_pwr_pwmled_driver_current_Big_step
    hal_pwr.o(i.hal_pwr_elvcc_vol_set) refers to drv_pwr.o(i.drv_pwr_hv_ldo_voltage_set) for drv_pwr_hv_ldo_voltage_set
    hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode) refers to drv_pwr.o(i.drv_pwr_set_wakeup_type) for drv_pwr_set_wakeup_type
    hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode) for drv_pwr_enter_deep_sleep_mode
    hal_pwr.o(i.hal_pwr_enter_normal_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_sleep_mode_ex) for drv_pwr_enter_sleep_mode_ex
    hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_stop_sleep_mode) for drv_pwr_enter_stop_sleep_mode
    hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) refers to hal_pwr.o(.data) for .data
    hal_pwr.o(i.hal_pwr_exit_sleep_mode) refers to drv_pwr.o(i.drv_pwr_exit_sleep_mode) for drv_pwr_exit_sleep_mode
    hal_pwr.o(i.hal_pwr_get_reset_flag) refers to drv_crgu.o(i.drv_crgu_get_all_reset_flag) for drv_crgu_get_all_reset_flag
    hal_pwr.o(i.hal_pwr_get_reset_flag) refers to drv_pwr.o(i.drv_pwr_get_wakeflag) for drv_pwr_get_wakeflag
    hal_pwr.o(i.hal_pwr_get_reset_flag) refers to drv_crgu.o(i.drv_crgu_clear_all_reset_flags) for drv_crgu_clear_all_reset_flags
    hal_pwr.o(i.hal_pwr_get_vcc_power_ready) refers to drv_pwr.o(i.drv_pwr_get_power_ready_st) for drv_pwr_get_power_ready_st
    hal_pwr.o(i.hal_pwr_ldo13s_en) refers to drv_pwr.o(i.drv_pwr_ldo13s_en) for drv_pwr_ldo13s_en
    hal_pwr.o(i.hal_pwr_ldo13s_set) refers to drv_pwr.o(i.drv_pwr_ldo13s_set) for drv_pwr_ldo13s_set
    hal_pwr.o(i.hal_pwr_ldo18s_en) refers to drv_pwr.o(i.drv_pwr_ldo18s_en) for drv_pwr_ldo18s_en
    hal_pwr.o(i.hal_pwr_ldo18s_set) refers to drv_pwr.o(i.drv_pwr_ldo18s_set) for drv_pwr_ldo18s_set
    hal_pwr.o(i.hal_pwr_set_main_power) refers to drv_pwr.o(i.drv_pwr_set_digit_power_sel) for drv_pwr_set_digit_power_sel
    hal_pwr.o(i.hal_pwr_set_pvd) refers to drv_pwr.o(i.drv_pwr_set_pvd) for drv_pwr_set_pvd
    hal_pwr.o(i.hal_pwr_set_sleep_mode_power) refers to drv_pwr.o(i.drv_pwr_set_breath_screen_power_sel) for drv_pwr_set_breath_screen_power_sel
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_ctrl_eint) for hal_gpio_ctrl_eint
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_init_eint) for hal_gpio_init_eint
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_reg_eint_cb) for hal_gpio_reg_eint_cb
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_pwr.o(.data) for .data
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_pwr.o(i.stop_sleep_cb) for stop_sleep_cb
    hal_pwr.o(i.hal_pwr_set_vcc_enable) refers to drv_pwr.o(i.drv_pwr_charge_pump_en) for drv_pwr_charge_pump_en
    hal_pwr.o(i.stop_sleep_cb) refers to hal_pwr.o(.data) for .data
    tau_delay.o(i.delayMs) refers to tau_delay.o(i.delayUs) for delayUs
    tau_delay.o(i.delayUs) refers to drv_common.o(.data) for g_system_delay_step
    tau_log.o(i.fgetc) refers to hal_uart.o(i.hal_uart_recv_blocking) for hal_uart_recv_blocking
    tau_log.o(i.fgetc) refers to hal_system.o(i.hal_system_get_debug_state) for hal_system_get_debug_state
    tau_log.o(i.fgetc) refers to hal_system.o(i.hal_system_clear_debug_state) for hal_system_clear_debug_state
    tau_log.o(i.fgetc) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.fputc) refers to tau_log.o(i.tau_log_push_log) for tau_log_push_log
    tau_log.o(i.fputc) refers to hal_uart.o(i.hal_uart_send_blocking) for hal_uart_send_blocking
    tau_log.o(i.fputc) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.tau_log_init) refers to hal_uart.o(i.hal_uart_init) for hal_uart_init
    tau_log.o(i.tau_log_init) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.tau_log_printf) refers to memseta.o(.text) for __aeabi_memclr4
    tau_log.o(i.tau_log_printf) refers to strlen.o(.text) for strlen
    tau_log.o(i.tau_log_printf) refers to printfa.o(i.__0vsprintf) for vsprintf
    tau_log.o(i.tau_log_printf) refers to tau_log.o(i.tau_log_push_log) for tau_log_push_log
    tau_log.o(i.tau_log_printf) refers to printfa.o(i.__0printf) for __2printf
    tau_log.o(i.tau_log_printf) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.tau_log_printf) refers to tau_log.o(.bss) for g_log_buf
    tau_log.o(i.tau_log_push_log) refers to memcpya.o(.text) for __aeabi_memcpy
    tau_log.o(i.tau_log_push_log) refers to tau_delay.o(i.delayUs) for delayUs
    tau_log.o(.ARM.__at_0x1101C) refers to tau_log.o(.bss) for g_log_buf
    hal_uart.o(i.hal_uart0_rx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart0_tx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart1_rx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart1_tx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_deinit) refers to drv_uart.o(i.drv_uart_deinit) for drv_uart_deinit
    hal_uart.o(i.hal_uart_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_uart.o(i.hal_uart_deinit) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_dma_path_close) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_uart.o(i.hal_uart_dma_path_close) refers to drv_dma.o(i.drv_dma_deinit) for drv_dma_deinit
    hal_uart.o(i.hal_uart_dma_path_close) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_apply_handle) for drv_dma_apply_handle
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_set_burst) for drv_dma_set_burst
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_register_callback) for drv_dma_register_callback
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_enable_int) for drv_dma_enable_int
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_set_mem_trans_info) for drv_dma_set_mem_trans_info
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_enable) for drv_dma_enable
    hal_uart.o(i.hal_uart_dma_recv) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_uart.o(i.hal_uart_dma_recv) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_dma_recv) refers to hal_uart.o(i.hal_uart0_rx_dma_cb) for hal_uart0_rx_dma_cb
    hal_uart.o(i.hal_uart_dma_recv) refers to hal_uart.o(i.hal_uart1_rx_dma_cb) for hal_uart1_rx_dma_cb
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_apply_handle) for drv_dma_apply_handle
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_set_burst) for drv_dma_set_burst
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_register_callback) for drv_dma_register_callback
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_enable_int) for drv_dma_enable_int
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_set_mem_trans_info) for drv_dma_set_mem_trans_info
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_enable) for drv_dma_enable
    hal_uart.o(i.hal_uart_dma_send) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_uart.o(i.hal_uart_dma_send) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_dma_send) refers to hal_uart.o(i.hal_uart0_tx_dma_cb) for hal_uart0_tx_dma_cb
    hal_uart.o(i.hal_uart_dma_send) refers to hal_uart.o(i.hal_uart1_tx_dma_cb) for hal_uart1_tx_dma_cb
    hal_uart.o(i.hal_uart_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_uart.o(i.hal_uart_init) refers to drv_uart.o(i.drv_uart_init) for drv_uart_init
    hal_uart.o(i.hal_uart_init) refers to drv_uart.o(i.drv_uart_trans_create_handle) for drv_uart_trans_create_handle
    hal_uart.o(i.hal_uart_init) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_init) refers to drv_common.o(.data) for g_system_clock
    hal_uart.o(i.hal_uart_init) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_recv_blocking) refers to drv_uart.o(i.drv_uart_recv_blocking) for drv_uart_recv_blocking
    hal_uart.o(i.hal_uart_recv_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_recv_none_blocking) refers to drv_uart.o(i.drv_uart_recv_none_blocking) for drv_uart_recv_none_blocking
    hal_uart.o(i.hal_uart_recv_none_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_send_blocking) refers to drv_uart.o(i.drv_uart_send_blocking) for drv_uart_send_blocking
    hal_uart.o(i.hal_uart_send_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_send_none_blocking) refers to drv_uart.o(i.drv_uart_send_none_blocking) for drv_uart_send_none_blocking
    hal_uart.o(i.hal_uart_send_none_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_internal_vsync.o(i.LCDC_IRQn_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.LCDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_internal_vsync.o(i.LCDC_IRQn_Handler) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) for hal_intl_fb_cal_fb_info
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) for hal_dsi_tx_ctrl_gen_a_tear_signal
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_delay.o(i.delayUs) for delayUs
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) for hal_vsync_reset_lcdc_scaler
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_sync_register_rx_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) for hal_intl_fb_set_fb_info_manual
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) for hal_intl_fb_cal_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_svs.o(i.hal_intl_svs_init_rx) for hal_intl_svs_init_rx
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr) for hal_intl_dcs_init_sw_fltr
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_rxbr.o(i.drv_rxbr_register_irq1_callback) for drv_rxbr_register_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_vidc.o(i.drv_vidc_register_callback) for drv_vidc_register_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_init) for dcs_packet_fifo_init
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_pro_motion_init) for soft_pro_motion_init
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_gen_te) for soft_gen_te
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.rxbr_irq1_callback) for rxbr_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.vidc_callback) for vidc_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_gen_te_double_buffer) for soft_gen_te_double_buffer
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) for hal_intl_fb_cal_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_svs.o(i.hal_intl_svs_deinit_rx) for hal_intl_svs_deinit_rx
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_svs.o(i.hal_intl_svs_set_sync_coef) for hal_intl_svs_set_sync_coef
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_memc.o(i.drv_memc_set_frame_drop_select) for drv_memc_set_frame_drop_select
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_set_tear_line) for drv_lcdc_set_tear_line
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to idiv.o(.text) for __aeabi_idivmod
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_config_acc_command_mode) for drv_lcdc_config_acc_command_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_svs.o(i.hal_intl_svs_deinit_tx) for hal_intl_svs_deinit_tx
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.soft_pro_motion_init) for soft_pro_motion_init
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_svs.o(i.hal_intl_svs_set_input_frate) for hal_intl_svs_set_input_frate
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg) for drv_rxbr_hline_rcv0_cfg
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dadd.o(.text) for __aeabi_dadd
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_internal_vsync.o(i.soft_pro_motion_init) for soft_pro_motion_init
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_int_source) for drv_rxbr_get_int_source
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.soft_double_buffer_update) for soft_double_buffer_update
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_svs.o(i.hal_intl_svs_handle) for hal_intl_svs_handle
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.vpre_err_reset) for vpre_err_reset
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_lcdc.o(i.drv_lcdc_cmd_start) for drv_lcdc_cmd_start
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt) for hal_intl_svs_set_rx_vtt
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.soft_double_buffer_update) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(i.soft_tear_adjust_line) for soft_tear_adjust_line
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.soft_gen_te_double_buffer) refers to hal_internal_vsync.o(i.soft_tear_adjust_line) for soft_tear_adjust_line
    hal_internal_vsync.o(i.soft_gen_te_double_buffer) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_pro_motion_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.soft_pro_motion_init) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_pro_motion_init) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.soft_tear_adjust_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_get_int_source) for drv_vidc_get_int_source
    hal_internal_vsync.o(i.vidc_callback) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_clear_irq) for drv_vidc_clear_irq
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_get_irq_status) for drv_vidc_get_irq_status
    hal_internal_vsync.o(i.vidc_callback) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.vpre_err_reset) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to hal_internal_dcs.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) for hal_intl_dcs_rx_receive_packet
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_dsc_dec.o(i.drv_dsc_dec_get_nslc) for drv_dsc_dec_get_nslc
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_crgu.o(i.drv_crgu_set_dsc_clk) for drv_crgu_set_dsc_clk
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to hal_internal_dcs.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr) refers to hal_internal_dcs.o(.bss) for .bss
    hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_register_write_cmd_entry) refers to hal_internal_dcs.o(.data) for .data
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle) for hal_intl_dcs_sw_filter_handle
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) for dcs_packet_fifo_alloc
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) for hal_dsi_rx_ctrl_dcs_async_handler
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_ddi_crc_en) for drv_dsi_rx_get_ddi_crc_en
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_dcs.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_dcs.o(.data) for .data
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) for hal_intl_dcs_rx_get_dcs_packet_data
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) for hal_intl_dcs_rx_receive_pps
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to hal_internal_dcs.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to memcmp.o(.text) for memcmp
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to hal_internal_dcs.o(.conststring) for .conststring
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) refers to memseta.o(.text) for __aeabi_memset
    hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) refers to drv_rxbr.o(i.drv_rxbr_set_filter_regs) for drv_rxbr_set_filter_regs
    hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) refers to hal_internal_dcs.o(.bss) for .bss
    hal_internal_dcs.o(i.hal_intl_dcs_set_dcs_direct_mode) refers to hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) for hal_intl_dcs_set_auto_hw_filter
    hal_internal_dcs.o(i.hal_intl_dcs_set_dcs_direct_mode) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle) refers to hal_internal_dcs.o(.data) for .data
    hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle) refers to hal_internal_dcs.o(.bss) for .bss
    hal_internal_dcs.o(.data) refers to hal_internal_dcs.o(.bss) for g_imm_buffer
    hal_internal_fb.o(i.ha_intl_fb_check_pu_size) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.ha_intl_fb_check_pu_size) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter) for hal_intl_fb_flow_control_adapter
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) for hal_intl_fb_check_bandwidth
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.ha_intl_fb_check_pu_size) for ha_intl_fb_check_pu_size
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.hal_intl_fb_edge_resize) for hal_intl_fb_edge_resize
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_fb.o(i.hal_intl_fb_edge_resize) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.hal_intl_fb_edge_resize) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_user_flow) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to hal_internal_fb.o(.conststring) for .conststring
    hal_internal_svs.o(i.hal_intl_svs_deinit_rx) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.hal_intl_svs_deinit_rx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_deinit_rx) refers to hal_internal_svs.o(i.svs_wait_start) for svs_wait_start
    hal_internal_svs.o(i.hal_intl_svs_deinit_tx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_handle) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) for hal_intl_svs_update_rxbr_clk
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_svs.o(i.svs_wait_start) for svs_wait_start
    hal_internal_svs.o(i.hal_intl_svs_init_tx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_svs.o(i.svs_wait_start) for svs_wait_start
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_svs.o(i.svs_wait_fr_stab) for svs_wait_fr_stab
    hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_set_sync_coef) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to dmul.o(.text) for __aeabi_dmul
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg) for drv_rxbr_hline_rcv1_cfg
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_get_rel_intv) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_svs.o(i.svs_get_rel_intv) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_sync_handle) refers to hal_internal_svs.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_svs.o(i.svs_sync_handle) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_svs.o(i.svs_sync_handle) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_svs.o(i.svs_sync_handle) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_svs.o(i.svs_sync_handle) refers to f2d.o(.text) for __aeabi_f2d
    hal_internal_svs.o(i.svs_sync_handle) refers to dadd.o(.text) for __aeabi_dadd
    hal_internal_svs.o(i.svs_sync_handle) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_svs.o(i.svs_sync_handle) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to hal_internal_svs.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to ffixui.o(.text) for __aeabi_f2uiz
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to hal_internal_svs.o(i.svs_sync_handle) for svs_sync_handle
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_svs.o(i.svs_wait_start) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_internal_svs.o(i.svs_wait_start) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_svs.o(i.svs_wait_start) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_internal_svs.o(i.svs_wait_start) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_svs.o(i.svs_wait_start) refers to f2d.o(.text) for __aeabi_f2d
    hal_internal_svs.o(i.svs_wait_start) refers to ceil.o(i.ceil) for ceil
    hal_internal_svs.o(i.svs_wait_start) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(i.svs_direct_mode_setting) for svs_direct_mode_setting
    hal_internal_svs.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_svs.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg) for drv_rxbr_hline_rcv1_cfg
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(i.svs_wait_fr_stab) for svs_wait_fr_stab
    drv_common.o(i.HardFault_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_common.o(i.SysTick_Handler) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_enable_systick) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_common.o(i.drv_common_enable_systick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_get_tick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_system_init) refers to drv_se.o(i.drv_se_init) for drv_se_init
    drv_common.o(i.drv_common_systick_register_cb) refers to drv_common.o(.data) for .data
    drv_crgu.o(i.drv_crgu_get_rxbr_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_crgu.o(i.drv_crgu_get_system_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to drv_se.o(i.drv_se_set_dsc) for drv_se_set_dsc
    drv_gpio.o(i.AP_NRESET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.AP_NRESET_IRQn_Handler) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.EXTI_INT0_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT1_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT2_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT3_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT4_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT5_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT6_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT7_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.drv_gpio_handle_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.drv_gpio_handle_int) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_register_ap_reset_callback) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.drv_gpio_register_callback) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_pwr.o(i.drv_pwr_analog_pwm_en) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_elvcc_pwm_en) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_elvcc_pwm_en) refers to tau_delay.o(i.delayMs) for delayMs
    drv_pwr.o(i.drv_pwr_enter_sleep_mode) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_enter_sleep_mode) refers to drv_pwr.o(i.drv_pwr_por_mode_flag) for drv_pwr_por_mode_flag
    drv_pwr.o(i.drv_pwr_enter_stop_sleep_mode) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_exit_sleep_mode) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_hv_ldo_mode_clock_sel) refers to drv_pwr.o(i.drv_pwr_hv_ldo_10M_clock) for drv_pwr_hv_ldo_10M_clock
    drv_pwr.o(i.drv_pwr_pwm_output_pwm_led) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_breath_screen_power_sel) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_digit_power_sel) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_system_clk) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_wakeup_type) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_swire.o(i.SWIRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_swire.o(i.SWIRE_IRQn_Handler) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_register_callback) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_sys_cfg.o(i.drv_sys_cfg_sel_dma_req) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_timer.o(i.TIMER0_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.TIMER1_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.TIMER2_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.TIMER3_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_timer.o(i.drv_timer_enable) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_get_instance) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_get_status) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_clear_status_flags) for drv_timer_clear_status_flags
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_register_callback) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_compare_val) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_compare_val) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_timer.o(i.drv_timer_set_compare_val) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_compare_val) refers to drv_common.o(.data) for g_system_clock
    drv_timer.o(i.drv_timer_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_repeat) refers to drv_timer.o(.data) for .data
    dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_fifo_init) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_size) refers to dcs_packet_fifo.o(.bss) for .bss
    drv_se.o(i.drv_se_init) refers to drv_efuse.o(i.drv_efuse_enter_inactive) for drv_efuse_enter_inactive
    drv_se.o(i.drv_se_init) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_se.o(i.drv_se_init) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_dsc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_dsc) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_lcdc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_lcdc) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_memc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_memc) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_rxbr) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_rxbr) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_vidc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_vidc) refers to drv_se.o(.data) for .data
    drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) refers to drv_dsi_rx.o(.data) for .data
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) for drv_dsi_rx_get_color_bpp
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to ffltui.o(.text) for __aeabi_ui2f
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fdiv.o(.text) for __aeabi_fdiv
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fmul.o(.text) for __aeabi_fmul
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc) for drv_dsi_rx_get_color_pcc
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fadd.o(.text) for __aeabi_fadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to cfrcmple.o(.text) for __aeabi_cfrcmple
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to f2d.o(.text) for __aeabi_f2d
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dadd.o(.text) for __aeabi_dadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dfixui.o(.text) for __aeabi_d2uiz
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_set_drv_log_level) refers to drv_dsi_rx.o(.data) for .data
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_test_lock) for drv_phy_test_lock
    drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_enter) for drv_tx_phy_test_enter
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_code) for drv_tx_phy_test_write_code
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_exit) for drv_tx_phy_test_exit
    drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_version) for drv_dsi_tx_version
    drv_dsi_tx.o(i.drv_dsi_tx_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_tx.o(i.drv_dsi_tx_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_lcdc.o(i.drv_lcdc_clear_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_lcdc.o(i.drv_lcdc_cmd_start) refers to drv_se.o(i.drv_se_set_lcdc) for drv_se_set_lcdc
    drv_lcdc.o(i.drv_lcdc_ctrl_flow) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    drv_lcdc.o(i.drv_lcdc_part_display_config) refers to drv_lcdc.o(i.drv_lcdc_pixel_value_config) for drv_lcdc_pixel_value_config
    drv_lcdc.o(i.drv_lcdc_set_int) refers to drv_lcdc.o(i.drv_lcdc_clear_int) for drv_lcdc_clear_int
    drv_lcdc.o(i.drv_lcdc_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_lcdc.o(i.drv_lcdc_vid_hw_start) refers to drv_se.o(i.drv_se_set_lcdc) for drv_se_set_lcdc
    drv_memc.o(i.MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_get_status) for drv_memc_get_status
    drv_memc.o(i.MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_clear_status) for drv_memc_clear_status
    drv_memc.o(i.MEMC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_memc.o(i.drv_memc_rate_transfer_sel) refers to drv_se.o(i.drv_se_set_memc) for drv_se_set_memc
    drv_memc.o(i.drv_memc_set_ltpo_mode) refers to drv_se.o(i.drv_se_set_memc) for drv_se_set_memc
    drv_rxbr.o(i.VPRE1_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.VPRE1_IRQn_Handler) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_EnableIRQ) for __NVIC_EnableIRQ
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_rxbr.o(i.drv_rxbr_register_irq0_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_register_irq1_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_set_cmd_filter) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_rxbr.o(i.drv_rxbr_set_cmd_response) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_rxbr.o(i.drv_rxbr_set_color_format) refers to drv_se.o(i.drv_se_set_rxbr) for drv_se_set_rxbr
    drv_rxbr.o(i.drv_rxbr_soft_reset) refers to tau_delay.o(i.delayMs) for delayMs
    drv_rxbr.o(i.drv_rxbr_sw_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_rxbr.o(i.drv_rxbr_sw_reset) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    drv_vidc.o(i.VIDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.VIDC_IRQn_Handler) refers to drv_vidc.o(.data) for .data
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_vidc.o(i.drv_vidc_register_callback) refers to drv_vidc.o(.data) for .data
    drv_vidc.o(i.drv_vidc_set_src_parameter) refers to drv_se.o(i.drv_se_set_vidc) for drv_se_set_vidc
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(i.drv_dma_get_int_source) for drv_dma_get_int_source
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(i.drv_dma_clear_status) for drv_dma_clear_status
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(.data) for .data
    drv_dma.o(i.drv_dma_apply_handle) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dma.o(i.drv_dma_apply_handle) refers to drv_dma.o(.data) for .data
    drv_dma.o(i.drv_dma_apply_handle) refers to drv_dma.o(.constdata) for .constdata
    drv_dma.o(i.drv_dma_deinit) refers to drv_dma.o(i.drv_dma_disable_int) for drv_dma_disable_int
    drv_dma.o(i.drv_dma_disable_int) refers to drv_dma.o(i.drv_dma_int_list_delete) for drv_dma_int_list_delete
    drv_dma.o(i.drv_dma_disable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.drv_dma_enable_int) refers to drv_dma.o(i.drv_dma_int_list_inset) for drv_dma_int_list_inset
    drv_dma.o(i.drv_dma_enable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dma.o(i.drv_dma_init) refers to drv_per_common.o(i.drv_per_set_clock) for drv_per_set_clock
    drv_dma.o(i.drv_dma_init) refers to drv_dma.o(i.drv_dma_update_handle_setting) for drv_dma_update_handle_setting
    drv_dma.o(i.drv_dma_int_list_delete) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_int_list_inset) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_update_handle_setting) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_dma_req) for drv_sys_cfg_sel_dma_req
    drv_dma.o(i.drv_dma_update_req_by_default) refers to drv_dma.o(i.drv_dma_update_handle_setting) for drv_dma_update_handle_setting
    drv_dma.o(i.drv_dma_update_req_by_default) refers to drv_dma.o(.constdata) for .constdata
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_int_trans_handle) for drv_uart_int_trans_handle
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_abort_recv) for drv_uart_abort_recv
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_abort_send) for drv_uart_abort_send
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(.constdata) for .constdata
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(i.drv_uart_reset_rx_fifo) for drv_uart_reset_rx_fifo
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(i.drv_uart_reset_tx_fifo) for drv_uart_reset_tx_fifo
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_deinit) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_deinit) refers to drv_uart.o(i.drv_uart_enable_clk) for drv_uart_enable_clk
    drv_uart.o(i.drv_uart_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.drv_uart_deinit) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_enable_clk) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    drv_uart.o(i.drv_uart_enable_int) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_enable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.drv_uart_get_def_cfg) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.drv_uart_get_def_cfg) refers to drv_common.o(.data) for g_system_clock
    drv_uart.o(i.drv_uart_get_instance) refers to drv_uart.o(.constdata) for .constdata
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_enable_clk) for drv_uart_enable_clk
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_set_baud_rate) for drv_uart_set_baud_rate
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_enable_int) for drv_uart_enable_int
    drv_uart.o(i.drv_uart_int_trans_handle) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_recv_none_blocking) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_recv_none_blocking) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_recv_none_blocking) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_reset_rx_fifo) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_reset_tx_fifo) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_send_none_blocking) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_send_none_blocking) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_send_none_blocking) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_set_baud_rate) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_uart.o(i.drv_uart_trans_create_handle) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_trans_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.drv_uart_trans_create_handle) refers to drv_uart.o(.bss) for .bss
    drv_efuse.o(i.drv_efuse_enter_inactive) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    drv_efuse.o(i.drv_efuse_enter_inactive) refers to drv_efuse.o(i.drv_efuse_int_enable) for drv_efuse_int_enable
    drv_efuse.o(i.drv_efuse_read) refers to drv_pwr.o(i.drv_pwr_efuse_pd) for drv_pwr_efuse_pd
    drv_efuse.o(i.drv_efuse_read) refers to drv_efuse.o(i.drv_efuse_read_req) for drv_efuse_read_req
    drv_efuse.o(i.drv_efuse_write) refers to drv_pwr.o(i.drv_pwr_efuse_pd) for drv_pwr_efuse_pd
    drv_efuse.o(i.drv_efuse_write) refers to drv_efuse.o(i.drv_efuse_write_req) for drv_efuse_write_req
    drv_efuse.o(i.drv_efuse_write_read_req_clear) refers to drv_efuse.o(i.drv_efuse_write_req) for drv_efuse_write_req
    drv_efuse.o(i.drv_efuse_write_read_req_clear) refers to drv_efuse.o(i.drv_efuse_read_req) for drv_efuse_read_req
    drv_per_common.o(i.drv_per_get_system_clk) refers to drv_crgu.o(i.drv_crgu_get_system_clk) for drv_crgu_get_system_clk
    drv_per_common.o(i.drv_per_reset_module) refers to drv_crgu.o(i.drv_crgu_reset_modules) for drv_crgu_reset_modules
    drv_per_common.o(i.drv_per_set_clock) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    ceil.o(i.__softfp_ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.__softfp_ceil) refers to ceil.o(i.ceil) for ceil
    ceil.o(i.ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.ceil) refers to dadd.o(.text) for __aeabi_dadd
    ceil.o(i.ceil) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry10a.o(.ARM.Collect$$$$0000000D) for __rt_final_cpp
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry11a.o(.ARM.Collect$$$$0000000F) for __rt_final_exit
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry7b.o(.ARM.Collect$$$$00000008) for _main_clock
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry8b.o(.ARM.Collect$$$$0000000A) for _main_cpp_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry9a.o(.ARM.Collect$$$$0000000B) for _main_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry5.o(.ARM.Collect$$$$00000004) for _main_scatterload
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry2.o(.ARM.Collect$$$$00000001) for _main_stk
    idiv.o(.text) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfb.o(i.__0fprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0fprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0printf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printfb.o(i.__0vfprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vfprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printf0.o(i.__0fprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0fprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0printf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf0.o(i.__0vfprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vfprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf1.o(i.__0fprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0fprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0printf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i.__0vfprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vfprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf2.o(i.__0fprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0fprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0printf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf2.o(i.__0vfprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vfprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf3.o(i.__0fprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0fprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0printf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i.__0vfprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vfprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf4.o(i.__0fprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0fprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0printf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i.__0vfprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vfprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf5.o(i.__0fprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0fprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0printf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i.__0vfprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vfprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf6.o(i.__0fprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0fprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0printf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i.__0vfprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vfprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i._printf_core) refers to printf6.o(i._printf_pre_padding) for _printf_pre_padding
    printf6.o(i._printf_core) refers to printf6.o(i._printf_post_padding) for _printf_post_padding
    printf6.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf7.o(i.__0fprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0fprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0printf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i.__0vfprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vfprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i._printf_core) refers to printf7.o(i._printf_pre_padding) for _printf_pre_padding
    printf7.o(i._printf_core) refers to printf7.o(i._printf_post_padding) for _printf_post_padding
    printf7.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf8.o(i.__0fprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0fprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0printf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i.__0vfprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vfprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i._printf_core) refers to printf8.o(i._printf_pre_padding) for _printf_pre_padding
    printf8.o(i._printf_core) refers to printf8.o(i._printf_post_padding) for _printf_post_padding
    printf8.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i.__0fprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0fprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0fprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0printf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0printf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0snprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0snprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0snprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0sprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0sprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0sprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i.__0vfprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vfprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vfprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0vsnprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0vsprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i._fp_digits) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._fp_digits) refers to dmul.o(.text) for __aeabi_dmul
    printfa.o(i._fp_digits) refers to ddiv.o(.text) for __aeabi_ddiv
    printfa.o(i._fp_digits) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    printfa.o(i._fp_digits) refers to dadd.o(.text) for __aeabi_dadd
    printfa.o(i._fp_digits) refers to dfixul.o(.text) for __aeabi_d2ulz
    printfa.o(i._fp_digits) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_core) refers to printfa.o(i._printf_pre_padding) for _printf_pre_padding
    printfa.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers to printfa.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i._printf_core) refers to printfa.o(i._fp_digits) for _fp_digits
    printfa.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfa.o(i._printf_post_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_pre_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._snputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._sputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    fmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers to fepilogue.o(.text) for _float_round
    fscalb.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    dadd.o(.text) refers to llsshr.o(.text) for __aeabi_lasr
    dadd.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dmul.o(.text) refers to depilogue.o(.text) for _double_epilogue
    fflti.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fflti.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    ffltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ffltui.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    dfltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfltui.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ffixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixui.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    f2d.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    d2f.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    d2f.o(.text) refers to fepilogue.o(.text) for _float_round
    cfcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    cfrcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    entry2.o(.ARM.Collect$$$$00000001) refers to entry2.o(.ARM.Collect$$$$00002712) for __lit__00000000
    entry2.o(.ARM.Collect$$$$00002712) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    entry5.o(.ARM.Collect$$$$00000004) refers to init.o(.text) for __scatterload
    entry9a.o(.ARM.Collect$$$$0000000B) refers to main.o(i.main) for main
    entry9b.o(.ARM.Collect$$$$0000000C) refers to main.o(i.main) for main
    uldiv.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    uldiv.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to depilogue.o(i.__ARM_clz) for __ARM_clz
    depilogue.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    ddiv.o(.text) refers to depilogue.o(.text) for _double_round
    dfixul.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixul.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    init.o(.text) refers to entry5.o(.ARM.Collect$$$$00000004) for __main_after_scatterload


==============================================================================

Removing Unused input sections from the image.

    Removing main.o(.rev16_text), (4 bytes).
    Removing main.o(.revsh_text), (4 bytes).
    Removing p6a_demo.o(.rev16_text), (4 bytes).
    Removing p6a_demo.o(.revsh_text), (4 bytes).
    Removing p6a_demo.o(i.Gpio_swire_output), (80 bytes).
    Removing p6a_demo.o(i.Panel_CCM), (42 bytes).
    Removing p6a_demo.o(i.ap_dcs_set_exit_idle_mode), (100 bytes).
    Removing p6a_demo.o(i.ap_dcs_set_frame_change), (52 bytes).
    Removing p6a_demo.o(i.ap_set_FPS_B1), (74 bytes).
    Removing p6a_demo.o(i.soft_te_timer_cb), (28 bytes).
    Removing p6a_demo.o(i.soft_te_timer_init), (40 bytes).
    Removing board.o(.rev16_text), (4 bytes).
    Removing board.o(.revsh_text), (4 bytes).
    Removing startup_armcm0.o(HEAP), (3072 bytes).
    Removing hal_dsi_rx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd), (220 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_short_cmd), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_line), (604 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init), (320 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern), (256 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_force_video_crtl), (12 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_cap_pixel_color), (10 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en), (8 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback), (52 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_write_cmd_entry), (10 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle), (40 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart), (68 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack), (176 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cap_pixel_pos), (10 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_check_crc), (24 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk), (32 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter), (44 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_log_level), (8 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data), (240 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data_ex), (392 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk), (72 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk), (56 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate), (10 bytes).
    Removing hal_dsi_rx_ctrl.o(i.swap_uint16_t), (10 bytes).
    Removing hal_dsi_tx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode), (112 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick), (244 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_frame), (12 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_get_disp_line), (12 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_overwrite_enable), (22 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_partial_disp_enable), (70 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd), (128 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle), (32 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs), (60 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm), (8 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_sync_line), (36 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect), (60 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance), (60 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness), (12 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div), (52 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc), (60 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg), (28 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera), (68 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd), (244 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update), (16 bytes).
    Removing hal_gpio.o(.rev16_text), (4 bytes).
    Removing hal_gpio.o(.revsh_text), (4 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_input_data), (18 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_int_type), (20 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_pull_state), (40 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_driving_strength), (44 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_high_impedance), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_pull_state), (72 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_schmitt_trigger), (52 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_slew_rate), (52 bytes).
    Removing hal_swire.o(.rev16_text), (4 bytes).
    Removing hal_swire.o(.revsh_text), (4 bytes).
    Removing hal_swire.o(i.hal_swire_register_callback), (22 bytes).
    Removing hal_swire.o(i.hal_swire_set_waveform), (92 bytes).
    Removing hal_system.o(.rev16_text), (4 bytes).
    Removing hal_system.o(.revsh_text), (4 bytes).
    Removing hal_system.o(i.hal_system_clear_debug_state), (10 bytes).
    Removing hal_system.o(i.hal_system_disable_systick), (8 bytes).
    Removing hal_system.o(i.hal_system_enable_systick), (8 bytes).
    Removing hal_system.o(i.hal_system_get_debug_state), (8 bytes).
    Removing hal_system.o(i.hal_system_get_tick), (8 bytes).
    Removing hal_system.o(i.hal_system_idle_mode), (8 bytes).
    Removing hal_system.o(i.hal_system_register_systick_cb), (8 bytes).
    Removing hal_system.o(i.hal_system_reset_chip), (10 bytes).
    Removing hal_timer.o(.rev16_text), (4 bytes).
    Removing hal_timer.o(.revsh_text), (4 bytes).
    Removing hal_timer.o(i.hal_timer_get_status), (8 bytes).
    Removing hal_timer.o(i.hal_timer_start), (48 bytes).
    Removing hal_timer.o(i.hal_timer_start_ex), (42 bytes).
    Removing hal_timer.o(i.hal_timer_stop), (40 bytes).
    Removing hal_pwr.o(.rev16_text), (4 bytes).
    Removing hal_pwr.o(.revsh_text), (4 bytes).
    Removing hal_pwr.o(i.hal_pwr_elvcc_close), (10 bytes).
    Removing hal_pwr.o(i.hal_pwr_elvcc_ldo_en), (46 bytes).
    Removing hal_pwr.o(i.hal_pwr_elvcc_vol_set), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_get_reset_flag), (66 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo13s_en), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo13s_set), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo18s_en), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo18s_set), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_set_pvd), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_set_vcc_enable), (8 bytes).
    Removing tau_delay.o(.rev16_text), (4 bytes).
    Removing tau_delay.o(.revsh_text), (4 bytes).
    Removing tau_log.o(.rev16_text), (4 bytes).
    Removing tau_log.o(.revsh_text), (4 bytes).
    Removing tau_log.o(i.fgetc), (72 bytes).
    Removing hal_uart.o(.rev16_text), (4 bytes).
    Removing hal_uart.o(.revsh_text), (4 bytes).
    Removing hal_uart.o(i.hal_uart0_rx_dma_cb), (20 bytes).
    Removing hal_uart.o(i.hal_uart0_tx_dma_cb), (36 bytes).
    Removing hal_uart.o(i.hal_uart1_rx_dma_cb), (20 bytes).
    Removing hal_uart.o(i.hal_uart1_tx_dma_cb), (36 bytes).
    Removing hal_uart.o(i.hal_uart_deinit), (48 bytes).
    Removing hal_uart.o(i.hal_uart_dma_path_close), (92 bytes).
    Removing hal_uart.o(i.hal_uart_dma_recv), (276 bytes).
    Removing hal_uart.o(i.hal_uart_dma_send), (280 bytes).
    Removing hal_uart.o(i.hal_uart_recv_blocking), (28 bytes).
    Removing hal_uart.o(i.hal_uart_recv_none_blocking), (28 bytes).
    Removing hal_uart.o(i.hal_uart_send_none_blocking), (28 bytes).
    Removing hal_internal_vsync.o(.rev16_text), (4 bytes).
    Removing hal_internal_vsync.o(.revsh_text), (4 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te), (2 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_register_rx_callback), (28 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual), (28 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line), (60 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate), (134 bytes).
    Removing hal_internal_vsync.o(.data), (4 bytes).
    Removing hal_internal_dcs.o(.rev16_text), (4 bytes).
    Removing hal_internal_dcs.o(.revsh_text), (4 bytes).
    Removing hal_internal_dcs.o(i.hal_intl_dcs_register_write_cmd_entry), (12 bytes).
    Removing hal_internal_dcs.o(i.hal_intl_dcs_set_dcs_direct_mode), (44 bytes).
    Removing hal_internal_fb.o(.rev16_text), (4 bytes).
    Removing hal_internal_fb.o(.revsh_text), (4 bytes).
    Removing hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual), (480 bytes).
    Removing hal_internal_fb.o(.conststring), (152 bytes).
    Removing hal_internal_svs.o(.rev16_text), (4 bytes).
    Removing hal_internal_svs.o(.revsh_text), (4 bytes).
    Removing hal_internal_svs.o(i.hal_intl_svs_set_input_frate), (112 bytes).
    Removing hal_internal_svs.o(i.hal_intl_svs_set_sync_coef), (12 bytes).
    Removing drv_common.o(.rev16_text), (4 bytes).
    Removing drv_common.o(.revsh_text), (4 bytes).
    Removing drv_common.o(i.drv_common_disable_systick), (20 bytes).
    Removing drv_common.o(i.drv_common_enable_systick), (88 bytes).
    Removing drv_common.o(i.drv_common_get_tick), (12 bytes).
    Removing drv_common.o(i.drv_common_idle_mode), (40 bytes).
    Removing drv_common.o(i.drv_common_systick_register_cb), (12 bytes).
    Removing drv_crgu.o(.rev16_text), (4 bytes).
    Removing drv_crgu.o(.revsh_text), (4 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_all_reset_flags), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_reset_flag), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_all_reset_flag), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_reset_flag), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_system_clk), (104 bytes).
    Removing drv_crgu.o(i.drv_crgu_reset_chip), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_clock_src), (16 bytes).
    Removing drv_dsc_dec.o(.rev16_text), (4 bytes).
    Removing drv_dsc_dec.o(.revsh_text), (4 bytes).
    Removing drv_gpio.o(.rev16_text), (4 bytes).
    Removing drv_gpio.o(.revsh_text), (4 bytes).
    Removing drv_gpio.o(i.drv_gpio_get_attribute), (16 bytes).
    Removing drv_gpio.o(i.drv_gpio_get_input_data), (24 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_attribute), (28 bytes).
    Removing drv_pwr.o(.rev16_text), (4 bytes).
    Removing drv_pwr.o(.revsh_text), (4 bytes).
    Removing drv_pwr.o(i.drv_pwr_10bit_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_analog_pwm_en), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_charge_pump_en), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_close_iov18_tp18), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_dsc_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_elvcc_pwm_en), (124 bytes).
    Removing drv_pwr.o(i.drv_pwr_enter_sleep_mode), (152 bytes).
    Removing drv_pwr.o(i.drv_pwr_exit_sleep_mode_ex), (40 bytes).
    Removing drv_pwr.o(i.drv_pwr_fb_pd), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_get_wakeflag), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_get_write_lock_st), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_hf_frm_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_10M_clock), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_mode_clock_sel), (60 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_mode_sel), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_voltage_set), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo11d_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo13s_en), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo13s_set), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo15_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo18s_en), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo18s_set), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_ltpo_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_osc32k_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_osc80m_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_p3k_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_por_mode_flag), (32 bytes).
    Removing drv_pwr.o(i.drv_pwr_power_in), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_power_ready_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_power_sel), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwm_output_pwm_led), (56 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_driver_current_Big_step), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_driver_current_small_step), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_electric_current), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_open_drain), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_ram_pd_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_read_boot_chipst), (12 bytes).
    Removing drv_pwr.o(i.drv_pwr_read_chipcfg), (12 bytes).
    Removing drv_pwr.o(i.drv_pwr_rgbr_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_ap_rst_mode), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_ldo11_mode), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_ldo15_mode), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_pvd), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_pvd_mode), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_system_clk), (32 bytes).
    Removing drv_pwr.o(i.drv_pwr_sw_tp18_en), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_wakeflag_get), (16 bytes).
    Removing drv_swire.o(.rev16_text), (4 bytes).
    Removing drv_swire.o(.revsh_text), (4 bytes).
    Removing drv_sys_cfg.o(.rev16_text), (4 bytes).
    Removing drv_sys_cfg.o(.revsh_text), (4 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_sel_dma_req), (128 bytes).
    Removing drv_timer.o(.rev16_text), (4 bytes).
    Removing drv_timer.o(.revsh_text), (4 bytes).
    Removing drv_timer.o(i.drv_timer_get_status), (38 bytes).
    Removing drv_timer.o(i.drv_timer_register_callback), (20 bytes).
    Removing dcs_packet_fifo.o(.rev16_text), (4 bytes).
    Removing dcs_packet_fifo.o(.revsh_text), (4 bytes).
    Removing dcs_packet_fifo.o(i.dcs_packet_get_fifo_size), (16 bytes).
    Removing drv_se.o(.rev16_text), (4 bytes).
    Removing drv_se.o(.revsh_text), (4 bytes).
    Removing drv_dsi_rx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_rx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_force_video_crtl), (28 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_lpdt_fifo_status), (16 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate), (68 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_version), (12 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg), (24 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_drv_log_level), (12 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg), (48 bytes).
    Removing drv_dsi_tx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_tx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_force_interrupt), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_get_phy_status), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_forcepll), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_start), (24 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot), (68 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger), (92 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter), (296 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit), (228 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_sdf_3d), (32 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_bta), (28 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_vpg), (100 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_version), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_vid_shadow), (20 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_clear), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_lock), (32 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_read), (16 bytes).
    Removing drv_lcdc.o(.rev16_text), (4 bytes).
    Removing drv_lcdc.o(.revsh_text), (4 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_clear_irq), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_dpisignal_output_ctrl), (44 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_fixed_frame_output), (56 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_dpbuf_num), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_dpi_status), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_frame_clk_count), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_int_en_status), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_int_status), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_line_status), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_rgb2pen_subpixel), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_part_display_config), (52 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_pixel_value_config), (32 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_rd_st_line_config), (28 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_software_reset), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_update_shadow_reg), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_vid_sw_start), (56 bytes).
    Removing drv_memc.o(.rev16_text), (4 bytes).
    Removing drv_memc.o(.revsh_text), (4 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_frm_time), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_int_frame), (36 bytes).
    Removing drv_memc.o(i.drv_memc_set_double_buffer_reverse), (24 bytes).
    Removing drv_memc.o(i.drv_memc_set_fb_pri), (44 bytes).
    Removing drv_memc.o(i.drv_memc_set_fb_remaining_line_trigger), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_inten), (28 bytes).
    Removing drv_memc.o(i.drv_memc_set_read_trigger_line), (24 bytes).
    Removing drv_memc.o(i.drv_memc_set_te_ind), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_tear_hwclr), (24 bytes).
    Removing drv_memc.o(i.drv_memc_set_vidc_fb_arb), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_write_trigger_line), (24 bytes).
    Removing drv_rxbr.o(.rev16_text), (4 bytes).
    Removing drv_rxbr.o(.revsh_text), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_clr_swp_cnt), (16 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_dsc_flush), (24 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_col_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_cur_hline_rcv_cnt), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_frame_data_interval), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_hline_dcat), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_ipi_vsync_interval), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_page_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_pix_fmt), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_swpxl_cnt), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg), (20 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_register_irq0_callback), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_ack_pkt_md), (28 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_cmd_filter), (320 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_cmd_response), (324 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_col_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_compress), (32 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_data_catch_hline), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_page_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_swpxl_data), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_tmpdith_bp), (28 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_soft_reset), (32 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_sw_reset), (164 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_swpxl_clr), (32 bytes).
    Removing drv_vidc.o(.rev16_text), (4 bytes).
    Removing drv_vidc.o(.revsh_text), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_clear_status0), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_cap_pixel), (28 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_signal_frame), (36 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status0), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status1), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status2), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_dsc_thresh), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_frmst_latency), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_inff_thresh), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_irq_line), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_module_enable), (28 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_outff_thresh), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_update_src_format), (20 bytes).
    Removing drv_dma.o(.rev16_text), (4 bytes).
    Removing drv_dma.o(.revsh_text), (4 bytes).
    Removing drv_dma.o(i.drv_dma_apply_handle), (304 bytes).
    Removing drv_dma.o(i.drv_dma_deinit), (52 bytes).
    Removing drv_dma.o(i.drv_dma_disable), (20 bytes).
    Removing drv_dma.o(i.drv_dma_disable_int), (40 bytes).
    Removing drv_dma.o(i.drv_dma_enable), (36 bytes).
    Removing drv_dma.o(i.drv_dma_enable_int), (68 bytes).
    Removing drv_dma.o(i.drv_dma_get_remaining_trans_num), (20 bytes).
    Removing drv_dma.o(i.drv_dma_get_status), (20 bytes).
    Removing drv_dma.o(i.drv_dma_init), (22 bytes).
    Removing drv_dma.o(i.drv_dma_int_list_delete), (88 bytes).
    Removing drv_dma.o(i.drv_dma_int_list_inset), (48 bytes).
    Removing drv_dma.o(i.drv_dma_register_callback), (4 bytes).
    Removing drv_dma.o(i.drv_dma_reset), (36 bytes).
    Removing drv_dma.o(i.drv_dma_set_bitwide), (56 bytes).
    Removing drv_dma.o(i.drv_dma_set_burst), (20 bytes).
    Removing drv_dma.o(i.drv_dma_set_circle_mode), (40 bytes).
    Removing drv_dma.o(i.drv_dma_set_dir), (40 bytes).
    Removing drv_dma.o(i.drv_dma_set_increment), (72 bytes).
    Removing drv_dma.o(i.drv_dma_set_mem_trans_info), (40 bytes).
    Removing drv_dma.o(i.drv_dma_set_mem_trans_offset), (24 bytes).
    Removing drv_dma.o(i.drv_dma_set_per_address), (20 bytes).
    Removing drv_dma.o(i.drv_dma_set_priority), (32 bytes).
    Removing drv_dma.o(i.drv_dma_set_tran_int_cnt), (28 bytes).
    Removing drv_dma.o(i.drv_dma_update_handle_setting), (148 bytes).
    Removing drv_dma.o(i.drv_dma_update_req_by_default), (40 bytes).
    Removing drv_dma.o(.constdata), (136 bytes).
    Removing drv_uart.o(.rev16_text), (4 bytes).
    Removing drv_uart.o(.revsh_text), (4 bytes).
    Removing drv_uart.o(i.drv_uart_deinit), (60 bytes).
    Removing drv_uart.o(i.drv_uart_get_def_cfg), (72 bytes).
    Removing drv_uart.o(i.drv_uart_recv_blocking), (48 bytes).
    Removing drv_uart.o(i.drv_uart_recv_none_blocking), (60 bytes).
    Removing drv_uart.o(i.drv_uart_send_none_blocking), (60 bytes).
    Removing drv_efuse.o(.rev16_text), (4 bytes).
    Removing drv_efuse.o(.revsh_text), (4 bytes).
    Removing drv_efuse.o(i.drv_efuse_crc_cal), (128 bytes).
    Removing drv_efuse.o(i.drv_efuse_get_default_config), (26 bytes).
    Removing drv_efuse.o(i.drv_efuse_int_disable), (12 bytes).
    Removing drv_efuse.o(i.drv_efuse_write), (56 bytes).
    Removing drv_efuse.o(i.drv_efuse_write_read_req_clear), (22 bytes).
    Removing drv_efuse.o(i.drv_efuse_write_req), (22 bytes).
    Removing drv_phy_common.o(.rev16_text), (4 bytes).
    Removing drv_phy_common.o(.revsh_text), (4 bytes).
    Removing drv_per_common.o(.rev16_text), (4 bytes).
    Removing drv_per_common.o(.revsh_text), (4 bytes).
    Removing drv_per_common.o(i.drv_per_get_system_clk), (8 bytes).
    Removing drv_per_common.o(i.drv_per_reset_module), (14 bytes).
    Removing drv_per_common.o(i.drv_per_set_clock), (14 bytes).
    Removing fflti.o(.text), (22 bytes).

381 unused section(s) (total 18794 bytes) removed from the image.

==============================================================================

Image Symbol Table

    Local Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    ../clib/../cmprslib/zerorunl2.c          0x00000000   Number         0  __dczerorl2.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uidiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  idiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uldiv.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry5.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry2.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llshl.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llushr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llsshr.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf7.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf6.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf5.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf3.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf4.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf2.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfb.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf0.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf1.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfa.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf8.o ABSOLUTE
    ../clib/microlib/printf/stubs.s          0x00000000   Number         0  stubs.o ABSOLUTE
    ../clib/microlib/stdio/streams.c         0x00000000   Number         0  stdout.o ABSOLUTE
    ../clib/microlib/string/memcmp.c         0x00000000   Number         0  memcmp.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpya.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpyb.o ABSOLUTE
    ../clib/microlib/string/memset.c         0x00000000   Number         0  memseta.o ABSOLUTE
    ../clib/microlib/string/strlen.c         0x00000000   Number         0  strlen.o ABSOLUTE
    ../clib/microlib/stubs.s                 0x00000000   Number         0  iusefp.o ABSOLUTE
    ../fplib/microlib/d2f.c                  0x00000000   Number         0  d2f.o ABSOLUTE
    ../fplib/microlib/f2d.c                  0x00000000   Number         0  f2d.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  dadd.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  fadd.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  ddiv.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  fdiv.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  fepilogue.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  depilogue.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixul.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixui.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  ffixui.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  fflti.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  dfltui.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  ffltui.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  dmul.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  fmul.o ABSOLUTE
    ../fplib/microlib/fpscalb.c              0x00000000   Number         0  fscalb.o ABSOLUTE
    ../mathlib/ceil.c                        0x00000000   Number         0  ceil.o ABSOLUTE
    ..\..\..\src\common\tau_delay.c          0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\..\..\src\common\tau_log.c            0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_per_common.c 0x00000000   Number         0  drv_per_common.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_pwr.c 0x00000000   Number         0  hal_pwr.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_swire.c 0x00000000   Number         0  hal_swire.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_timer.c 0x00000000   Number         0  hal_timer.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\dcs_packet_fifo.c 0x00000000   Number         0  dcs_packet_fifo.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_dcs.c 0x00000000   Number         0  hal_internal_dcs.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_fb.c 0x00000000   Number         0  hal_internal_fb.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_svs.c 0x00000000   Number         0  hal_internal_svs.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\src\drv_se.c  0x00000000   Number         0  drv_se.o ABSOLUTE
    ..\..\src\app\P6A\p6a_demo.c             0x00000000   Number         0  p6a_demo.o ABSOLUTE
    ..\..\src\app\main.c                     0x00000000   Number         0  main.o ABSOLUTE
    ..\..\src\board\board.c                  0x00000000   Number         0  board.o ABSOLUTE
    ..\..\src\board\startup\startup_ARMCM0.s 0x00000000   Number         0  startup_armcm0.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_delay.c     0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_log.c       0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_per_common.c 0x00000000   Number         0  drv_per_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_pwr.c 0x00000000   Number         0  hal_pwr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_swire.c 0x00000000   Number         0  hal_swire.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_timer.c 0x00000000   Number         0  hal_timer.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\dcs_packet_fifo.c 0x00000000   Number         0  dcs_packet_fifo.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_dcs.c 0x00000000   Number         0  hal_internal_dcs.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_fb.c 0x00000000   Number         0  hal_internal_fb.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_svs.c 0x00000000   Number         0  hal_internal_svs.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\src\\drv_se.c 0x00000000   Number         0  drv_se.o ABSOLUTE
    ..\\..\\src\\app\\P6A\\p6a_demo.c        0x00000000   Number         0  p6a_demo.o ABSOLUTE
    ..\\..\\src\\app\\main.c                 0x00000000   Number         0  main.o ABSOLUTE
    ..\\..\\src\\board\\board.c              0x00000000   Number         0  board.o ABSOLUTE
    cdrcmple.s                               0x00000000   Number         0  cdrcmple.o ABSOLUTE
    cfcmple.s                                0x00000000   Number         0  cfcmple.o ABSOLUTE
    cfrcmple.s                               0x00000000   Number         0  cfrcmple.o ABSOLUTE
    dc.s                                     0x00000000   Number         0  dc.o ABSOLUTE
    handlers.s                               0x00000000   Number         0  handlers.o ABSOLUTE
    init.s                                   0x00000000   Number         0  init.o ABSOLUTE
    RESET                                    0x00010000   Section      192  startup_armcm0.o(RESET)
    .ARM.Collect$$$$00000000                 0x000100c0   Section        0  entry.o(.ARM.Collect$$$$00000000)
    .ARM.Collect$$$$00000001                 0x000100c0   Section        4  entry2.o(.ARM.Collect$$$$00000001)
    .ARM.Collect$$$$00000004                 0x000100c4   Section        4  entry5.o(.ARM.Collect$$$$00000004)
    .ARM.Collect$$$$00000008                 0x000100c8   Section        0  entry7b.o(.ARM.Collect$$$$00000008)
    .ARM.Collect$$$$0000000A                 0x000100c8   Section        0  entry8b.o(.ARM.Collect$$$$0000000A)
    .ARM.Collect$$$$0000000B                 0x000100c8   Section        8  entry9a.o(.ARM.Collect$$$$0000000B)
    .ARM.Collect$$$$0000000D                 0x000100d0   Section        0  entry10a.o(.ARM.Collect$$$$0000000D)
    .ARM.Collect$$$$0000000F                 0x000100d0   Section        0  entry11a.o(.ARM.Collect$$$$0000000F)
    .ARM.Collect$$$$00002712                 0x000100d0   Section        4  entry2.o(.ARM.Collect$$$$00002712)
    __lit__00000000                          0x000100d0   Data           4  entry2.o(.ARM.Collect$$$$00002712)
    .text                                    0x000100d4   Section      120  startup_armcm0.o(.text)
    .text                                    0x0001014c   Section        0  uidiv.o(.text)
    .text                                    0x00010178   Section        0  idiv.o(.text)
    .text                                    0x000101a0   Section        0  memcpya.o(.text)
    .text                                    0x000101c4   Section        0  memseta.o(.text)
    .text                                    0x000101e8   Section        0  strlen.o(.text)
    .text                                    0x000101f6   Section        0  memcmp.o(.text)
    .text                                    0x00010210   Section        0  fadd.o(.text)
    .text                                    0x000102c2   Section        0  fmul.o(.text)
    .text                                    0x0001033c   Section        0  fdiv.o(.text)
    .text                                    0x000103b8   Section        0  fscalb.o(.text)
    .text                                    0x000103d0   Section        0  dadd.o(.text)
    .text                                    0x00010534   Section        0  dmul.o(.text)
    .text                                    0x00010604   Section        0  ffltui.o(.text)
    .text                                    0x00010614   Section        0  dfltui.o(.text)
    .text                                    0x00010630   Section        0  ffixui.o(.text)
    .text                                    0x00010658   Section        0  dfixui.o(.text)
    .text                                    0x00010694   Section        0  f2d.o(.text)
    .text                                    0x000106bc   Section        0  d2f.o(.text)
    .text                                    0x000106f4   Section       20  cfcmple.o(.text)
    .text                                    0x00010708   Section       20  cfrcmple.o(.text)
    .text                                    0x0001071c   Section        0  uldiv.o(.text)
    .text                                    0x0001077c   Section        0  llshl.o(.text)
    .text                                    0x0001079c   Section        0  llushr.o(.text)
    .text                                    0x000107be   Section        0  llsshr.o(.text)
    .text                                    0x000107e4   Section        0  iusefp.o(.text)
    .text                                    0x000107e4   Section        0  fepilogue.o(.text)
    .text                                    0x00010866   Section        0  depilogue.o(.text)
    .text                                    0x00010924   Section        0  ddiv.o(.text)
    .text                                    0x00010a14   Section        0  dfixul.o(.text)
    .text                                    0x00010a54   Section       40  cdrcmple.o(.text)
    .text                                    0x00010a7c   Section       36  init.o(.text)
    .text                                    0x00010aa0   Section        0  __dczerorl2.o(.text)
    i.AP_NRESET_IRQn_Handler                 0x00010af8   Section        0  drv_gpio.o(i.AP_NRESET_IRQn_Handler)
    i.DMA_IRQn_Handler                       0x00010b14   Section        0  drv_dma.o(i.DMA_IRQn_Handler)
    i.EXTI_INT0_IRQn_Handler                 0x00010b70   Section        0  drv_gpio.o(i.EXTI_INT0_IRQn_Handler)
    i.EXTI_INT1_IRQn_Handler                 0x00010b7a   Section        0  drv_gpio.o(i.EXTI_INT1_IRQn_Handler)
    i.EXTI_INT2_IRQn_Handler                 0x00010b84   Section        0  drv_gpio.o(i.EXTI_INT2_IRQn_Handler)
    i.EXTI_INT3_IRQn_Handler                 0x00010b8e   Section        0  drv_gpio.o(i.EXTI_INT3_IRQn_Handler)
    i.EXTI_INT4_IRQn_Handler                 0x00010b98   Section        0  drv_gpio.o(i.EXTI_INT4_IRQn_Handler)
    i.EXTI_INT5_IRQn_Handler                 0x00010ba2   Section        0  drv_gpio.o(i.EXTI_INT5_IRQn_Handler)
    i.EXTI_INT6_IRQn_Handler                 0x00010bac   Section        0  drv_gpio.o(i.EXTI_INT6_IRQn_Handler)
    i.EXTI_INT7_IRQn_Handler                 0x00010bb6   Section        0  drv_gpio.o(i.EXTI_INT7_IRQn_Handler)
    i.HardFault_Handler                      0x00010bc0   Section        0  drv_common.o(i.HardFault_Handler)
    i.LCDC_IRQn_Handler                      0x00010c08   Section        0  hal_internal_vsync.o(i.LCDC_IRQn_Handler)
    i.MEMC_IRQn_Handler                      0x00010d08   Section        0  drv_memc.o(i.MEMC_IRQn_Handler)
    i.MIPI_TX_IRQn_Handler                   0x00010da4   Section        0  drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler)
    i.SWIRE_IRQn_Handler                     0x00010e5c   Section        0  drv_swire.o(i.SWIRE_IRQn_Handler)
    i.SysTick_Handler                        0x00010e8c   Section        0  drv_common.o(i.SysTick_Handler)
    i.TIMER0_IRQn_Handler                    0x00010ea4   Section        0  drv_timer.o(i.TIMER0_IRQn_Handler)
    i.TIMER1_IRQn_Handler                    0x00010eae   Section        0  drv_timer.o(i.TIMER1_IRQn_Handler)
    i.TIMER2_IRQn_Handler                    0x00010eb8   Section        0  drv_timer.o(i.TIMER2_IRQn_Handler)
    i.TIMER3_IRQn_Handler                    0x00010ec2   Section        0  drv_timer.o(i.TIMER3_IRQn_Handler)
    i.VIDC_IRQn_Handler                      0x00010ecc   Section        0  drv_vidc.o(i.VIDC_IRQn_Handler)
    i.VPRE1_IRQn_Handler                     0x00010ee8   Section        0  drv_rxbr.o(i.VPRE1_IRQn_Handler)
    i.VPRE_IRQn_Handler                      0x00010f04   Section        0  hal_internal_dcs.o(i.VPRE_IRQn_Handler)
    i.__0printf                              0x00010f70   Section        0  printfa.o(i.__0printf)
    i.__0vsprintf                            0x00010f90   Section        0  printfa.o(i.__0vsprintf)
    i.__ARM_clz                              0x00010fb4   Section        0  depilogue.o(i.__ARM_clz)
    i.__ARM_common_switch8                   0x00010fe2   Section        0  hal_dsi_rx_ctrl.o(i.__ARM_common_switch8)
    i.__scatterload_null                     0x00010ffc   Section        2  handlers.o(i.__scatterload_null)
    .ARM.__at_0x11000                        0x00011000   Section       28  drv_common.o(.ARM.__at_0x11000)
    .ARM.__at_0x1101C                        0x0001101c   Section       16  tau_log.o(.ARM.__at_0x1101C)
    .ARM.__at_0x1102C                        0x0001102c   Section       22  hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C)
    i.MIPI_RX_IRQn_Handler                   0x00011044   Section        0  drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler)
    i.UART_IRQn_Handler                      0x000113a8   Section        0  drv_uart.o(i.UART_IRQn_Handler)
    i.__NVIC_DisableIRQ                      0x00011528   Section        0  drv_rxbr.o(i.__NVIC_DisableIRQ)
    __NVIC_DisableIRQ                        0x00011529   Thumb Code    26  drv_rxbr.o(i.__NVIC_DisableIRQ)
    i.__NVIC_EnableIRQ                       0x00011548   Section        0  drv_rxbr.o(i.__NVIC_EnableIRQ)
    __NVIC_EnableIRQ                         0x00011549   Thumb Code    18  drv_rxbr.o(i.__NVIC_EnableIRQ)
    i.__scatterload_copy                     0x00011560   Section       14  handlers.o(i.__scatterload_copy)
    i.__scatterload_zeroinit                 0x0001156e   Section       14  handlers.o(i.__scatterload_zeroinit)
    i._fp_digits                             0x0001157c   Section        0  printfa.o(i._fp_digits)
    _fp_digits                               0x0001157d   Thumb Code   344  printfa.o(i._fp_digits)
    i._printf_core                           0x000116f0   Section        0  printfa.o(i._printf_core)
    _printf_core                             0x000116f1   Thumb Code  1754  printfa.o(i._printf_core)
    i._printf_post_padding                   0x00011ddc   Section        0  printfa.o(i._printf_post_padding)
    _printf_post_padding                     0x00011ddd   Thumb Code    32  printfa.o(i._printf_post_padding)
    i._printf_pre_padding                    0x00011dfc   Section        0  printfa.o(i._printf_pre_padding)
    _printf_pre_padding                      0x00011dfd   Thumb Code    44  printfa.o(i._printf_pre_padding)
    i._sputc                                 0x00011e28   Section        0  printfa.o(i._sputc)
    _sputc                                   0x00011e29   Thumb Code    10  printfa.o(i._sputc)
    i.ap_dcs_read                            0x00011e34   Section        0  p6a_demo.o(i.ap_dcs_read)
    ap_dcs_read                              0x00011e35   Thumb Code   280  p6a_demo.o(i.ap_dcs_read)
    i.ap_dcs_set_backlight                   0x00011f78   Section        0  p6a_demo.o(i.ap_dcs_set_backlight)
    ap_dcs_set_backlight                     0x00011f79   Thumb Code   176  p6a_demo.o(i.ap_dcs_set_backlight)
    i.ap_dcs_set_display_off                 0x00012068   Section        0  p6a_demo.o(i.ap_dcs_set_display_off)
    ap_dcs_set_display_off                   0x00012069   Thumb Code    34  p6a_demo.o(i.ap_dcs_set_display_off)
    i.ap_dcs_set_display_on                  0x000120b0   Section        0  p6a_demo.o(i.ap_dcs_set_display_on)
    ap_dcs_set_display_on                    0x000120b1   Thumb Code    40  p6a_demo.o(i.ap_dcs_set_display_on)
    i.ap_dcs_set_enter_sleep_mode            0x000120f4   Section        0  p6a_demo.o(i.ap_dcs_set_enter_sleep_mode)
    ap_dcs_set_enter_sleep_mode              0x000120f5   Thumb Code    94  p6a_demo.o(i.ap_dcs_set_enter_sleep_mode)
    i.ap_dcs_set_exit_sleep_mode             0x0001217c   Section        0  p6a_demo.o(i.ap_dcs_set_exit_sleep_mode)
    ap_dcs_set_exit_sleep_mode               0x0001217d   Thumb Code    28  p6a_demo.o(i.ap_dcs_set_exit_sleep_mode)
    i.ap_rstn_pull_down_cb                   0x000121bc   Section        0  p6a_demo.o(i.ap_rstn_pull_down_cb)
    ap_rstn_pull_down_cb                     0x000121bd   Thumb Code    40  p6a_demo.o(i.ap_rstn_pull_down_cb)
    i.ap_rstn_pull_high_cb                   0x00012210   Section        0  p6a_demo.o(i.ap_rstn_pull_high_cb)
    ap_rstn_pull_high_cb                     0x00012211   Thumb Code    22  p6a_demo.o(i.ap_rstn_pull_high_cb)
    i.app_display_init                       0x0001222c   Section        0  p6a_demo.o(i.app_display_init)
    i.app_gpio_init                          0x00012258   Section        0  p6a_demo.o(i.app_gpio_init)
    i.app_init_panel                         0x00012274   Section        0  p6a_demo.o(i.app_init_panel)
    app_init_panel                           0x00012275   Thumb Code 12972  p6a_demo.o(i.app_init_panel)
    i.app_mipi_rx_init                       0x00015520   Section        0  p6a_demo.o(i.app_mipi_rx_init)
    app_mipi_rx_init                         0x00015521   Thumb Code   238  p6a_demo.o(i.app_mipi_rx_init)
    i.app_mipi_tx_init                       0x0001564c   Section        0  p6a_demo.o(i.app_mipi_tx_init)
    app_mipi_tx_init                         0x0001564d   Thumb Code   222  p6a_demo.o(i.app_mipi_tx_init)
    i.app_mipi_tx_start                      0x00015758   Section        0  p6a_demo.o(i.app_mipi_tx_start)
    app_mipi_tx_start                        0x00015759   Thumb Code    72  p6a_demo.o(i.app_mipi_tx_start)
    i.app_system_process                     0x000157c8   Section        0  p6a_demo.o(i.app_system_process)
    app_system_process                       0x000157c9   Thumb Code    60  p6a_demo.o(i.app_system_process)
    i.app_system_resume                      0x00015834   Section        0  p6a_demo.o(i.app_system_resume)
    app_system_resume                        0x00015835   Thumb Code    30  p6a_demo.o(i.app_system_resume)
    i.app_system_suspend                     0x00015878   Section        0  p6a_demo.o(i.app_system_suspend)
    app_system_suspend                       0x00015879   Thumb Code   202  p6a_demo.o(i.app_system_suspend)
    i.app_tx_panel_reset                     0x00015a08   Section        0  p6a_demo.o(i.app_tx_panel_reset)
    app_tx_panel_reset                       0x00015a09   Thumb Code    46  p6a_demo.o(i.app_tx_panel_reset)
    i.board_Init                             0x00015a38   Section        0  board.o(i.board_Init)
    i.ceil                                   0x00015a50   Section        0  ceil.o(i.ceil)
    i.check_mipi_rx_tx_video_info            0x00015b18   Section        0  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    check_mipi_rx_tx_video_info              0x00015b19   Thumb Code    44  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    i.check_pkt_buf_rev                      0x00015b44   Section        0  hal_internal_dcs.o(i.check_pkt_buf_rev)
    check_pkt_buf_rev                        0x00015b45   Thumb Code    84  hal_internal_dcs.o(i.check_pkt_buf_rev)
    i.dcs_packet_fifo_alloc                  0x00015bcc   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    i.dcs_packet_fifo_init                   0x00015c24   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    i.dcs_packet_free_fifo_header            0x00015c3c   Section        0  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    i.dcs_packet_get_fifo_header             0x00015c80   Section        0  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    i.delayMs                                0x00015ca4   Section        0  tau_delay.o(i.delayMs)
    i.delayUs                                0x00015cbc   Section        0  tau_delay.o(i.delayUs)
    i.drv_common_system_init                 0x00015ce8   Section        0  drv_common.o(i.drv_common_system_init)
    i.drv_crgu_enable_clock                  0x00015cf0   Section        0  drv_crgu.o(i.drv_crgu_enable_clock)
    i.drv_crgu_get_rxbr_clk                  0x00015d2c   Section        0  drv_crgu.o(i.drv_crgu_get_rxbr_clk)
    i.drv_crgu_reset_modules                 0x00015d94   Section        0  drv_crgu.o(i.drv_crgu_reset_modules)
    i.drv_crgu_set_ahb_clk                   0x00015da4   Section        0  drv_crgu.o(i.drv_crgu_set_ahb_clk)
    i.drv_crgu_set_clock_div                 0x00015dcc   Section        0  drv_crgu.o(i.drv_crgu_set_clock_div)
    i.drv_crgu_set_dpi_clk                   0x00015ddc   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_clk)
    i.drv_crgu_set_dsc_clk                   0x00015e18   Section        0  drv_crgu.o(i.drv_crgu_set_dsc_clk)
    i.drv_crgu_set_fb_clk                    0x00015e50   Section        0  drv_crgu.o(i.drv_crgu_set_fb_clk)
    i.drv_crgu_set_lcdc_clk                  0x00015e78   Section        0  drv_crgu.o(i.drv_crgu_set_lcdc_clk)
    i.drv_crgu_set_reset                     0x00015ea0   Section        0  drv_crgu.o(i.drv_crgu_set_reset)
    i.drv_crgu_set_rxbr_clk                  0x00015eb8   Section        0  drv_crgu.o(i.drv_crgu_set_rxbr_clk)
    i.drv_crgu_set_vidc_clk                  0x00015ee0   Section        0  drv_crgu.o(i.drv_crgu_set_vidc_clk)
    i.drv_dma_clear_status                   0x00015f08   Section        0  drv_dma.o(i.drv_dma_clear_status)
    i.drv_dma_get_int_source                 0x00015f20   Section        0  drv_dma.o(i.drv_dma_get_int_source)
    drv_dma_get_int_source                   0x00015f21   Thumb Code    16  drv_dma.o(i.drv_dma_get_int_source)
    i.drv_dsc_dec_disable                    0x00015f34   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    i.drv_dsc_dec_enable                     0x00015f50   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    i.drv_dsc_dec_get_nslc                   0x00015f88   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    i.drv_dsc_dec_set_irqen                  0x00015fa8   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_set_irqen)
    i.drv_dsi_rx_calc_ipi_tx_delay           0x00015fc4   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    i.drv_dsi_rx_enable_irq                  0x000160d0   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    i.drv_dsi_rx_get_color_bpp               0x00016110   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    drv_dsi_rx_get_color_bpp                 0x00016111   Thumb Code    62  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    i.drv_dsi_rx_get_color_pcc               0x00016160   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    drv_dsi_rx_get_color_pcc                 0x00016161   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    i.drv_dsi_rx_get_compression_en          0x0001617c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    i.drv_dsi_rx_get_ddi_crc_en              0x0001618c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_ddi_crc_en)
    i.drv_dsi_rx_get_max_ret_size            0x0001619c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size)
    i.drv_dsi_rx_power_up                    0x000161a8   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    i.drv_dsi_rx_set_check_crc               0x000161c0   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc)
    i.drv_dsi_rx_set_ctrl_cfg                0x000161dc   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    i.drv_dsi_rx_set_ddi_cfg                 0x00016200   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    i.drv_dsi_rx_set_ddi_crc_en              0x00016210   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_crc_en)
    i.drv_dsi_rx_set_inten                   0x0001622c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    i.drv_dsi_rx_set_ipi_cfg                 0x00016238   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    i.drv_dsi_rx_set_ipi_ycbcr_frmt          0x00016248   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_ycbcr_frmt)
    i.drv_dsi_rx_set_lane_swap               0x00016264   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    i.drv_dsi_rx_set_resp_cnt                0x00016278   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    i.drv_dsi_rx_set_tear_resp_en            0x0001629c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_tear_resp_en)
    i.drv_dsi_rx_set_up_phy                  0x000162b8   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    i.drv_dsi_rx_shut_down                   0x000163b8   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    i.drv_dsi_tx_command_header              0x000163d0   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    i.drv_dsi_tx_command_mode_cfg            0x000163e8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    i.drv_dsi_tx_command_put_payload         0x00016440   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    i.drv_dsi_tx_config_eotp                 0x0001644c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    i.drv_dsi_tx_config_int                  0x0001646c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    i.drv_dsi_tx_dpi_lpcmd_time              0x00016478   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    i.drv_dsi_tx_dpi_mode                    0x00016488   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    i.drv_dsi_tx_dpi_polarity                0x00016498   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    i.drv_dsi_tx_edpi_cmd_size               0x000164bc   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    i.drv_dsi_tx_get_cmd_status              0x000164c8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    i.drv_dsi_tx_mode                        0x000164d4   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    i.drv_dsi_tx_phy_clock_lane_auto_lp      0x000164e0   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    i.drv_dsi_tx_phy_clock_lane_req_hs       0x000164fc   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    i.drv_dsi_tx_phy_lane_mode               0x0001651c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    i.drv_dsi_tx_phy_status_ready            0x0001652c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    i.drv_dsi_tx_phy_status_stopstate        0x00016594   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    i.drv_dsi_tx_phy_test_setup              0x000165d8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    i.drv_dsi_tx_phy_time_cfg                0x00016728   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    i.drv_dsi_tx_powerup                     0x00016748   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    i.drv_dsi_tx_response_mode               0x00016754   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    i.drv_dsi_tx_set_bta_ack                 0x00016778   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    i.drv_dsi_tx_set_esc_div                 0x00016794   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    i.drv_dsi_tx_set_int                     0x000167a8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    i.drv_dsi_tx_set_time_out_div            0x000167e8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    i.drv_dsi_tx_set_video_chunk             0x00016800   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    i.drv_dsi_tx_set_video_timing            0x00016814   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    i.drv_dsi_tx_shutdown                    0x00016838   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    i.drv_dsi_tx_timeout_cfg                 0x00016844   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    i.drv_dsi_tx_video_mode_cfg              0x00016870   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    i.drv_efuse_enter_inactive               0x00016958   Section        0  drv_efuse.o(i.drv_efuse_enter_inactive)
    i.drv_efuse_int_enable                   0x0001698e   Section        0  drv_efuse.o(i.drv_efuse_int_enable)
    i.drv_efuse_read                         0x0001699a   Section        0  drv_efuse.o(i.drv_efuse_read)
    i.drv_efuse_read_req                     0x000169d4   Section        0  drv_efuse.o(i.drv_efuse_read_req)
    i.drv_gpio_handle_int                    0x000169ec   Section        0  drv_gpio.o(i.drv_gpio_handle_int)
    drv_gpio_handle_int                      0x000169ed   Thumb Code    30  drv_gpio.o(i.drv_gpio_handle_int)
    i.drv_gpio_register_ap_reset_callback    0x00016a10   Section        0  drv_gpio.o(i.drv_gpio_register_ap_reset_callback)
    i.drv_gpio_register_callback             0x00016a1c   Section        0  drv_gpio.o(i.drv_gpio_register_callback)
    i.drv_gpio_set_int                       0x00016a30   Section        0  drv_gpio.o(i.drv_gpio_set_int)
    i.drv_gpio_set_ioe                       0x00016a74   Section        0  drv_gpio.o(i.drv_gpio_set_ioe)
    i.drv_gpio_set_mode                      0x00016a94   Section        0  drv_gpio.o(i.drv_gpio_set_mode)
    i.drv_gpio_set_output_data               0x00016aa8   Section        0  hal_gpio.o(i.drv_gpio_set_output_data)
    drv_gpio_set_output_data                 0x00016aa9   Thumb Code    26  hal_gpio.o(i.drv_gpio_set_output_data)
    i.drv_lcdc_bcsa_config                   0x00016ac8   Section        0  drv_lcdc.o(i.drv_lcdc_bcsa_config)
    i.drv_lcdc_cfg_int_frame                 0x00016af0   Section        0  drv_lcdc.o(i.drv_lcdc_cfg_int_frame)
    i.drv_lcdc_clear_int                     0x00016b1c   Section        0  drv_lcdc.o(i.drv_lcdc_clear_int)
    drv_lcdc_clear_int                       0x00016b1d   Thumb Code    20  drv_lcdc.o(i.drv_lcdc_clear_int)
    i.drv_lcdc_cmd_start                     0x00016b34   Section        0  drv_lcdc.o(i.drv_lcdc_cmd_start)
    i.drv_lcdc_config_acc_command_mode       0x00016b68   Section        0  drv_lcdc.o(i.drv_lcdc_config_acc_command_mode)
    i.drv_lcdc_config_int                    0x00016b7c   Section        0  drv_lcdc.o(i.drv_lcdc_config_int)
    i.drv_lcdc_config_int_single             0x00016bb4   Section        0  drv_lcdc.o(i.drv_lcdc_config_int_single)
    i.drv_lcdc_config_overwrite_rgb          0x00016bdc   Section        0  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    i.drv_lcdc_config_src_parameter          0x00016bf4   Section        0  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    i.drv_lcdc_crop_hact                     0x00016c44   Section        0  drv_lcdc.o(i.drv_lcdc_crop_hact)
    i.drv_lcdc_ctrl_flow                     0x00016c54   Section        0  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    i.drv_lcdc_dith_config                   0x00016c8c   Section        0  drv_lcdc.o(i.drv_lcdc_dith_config)
    i.drv_lcdc_edge_dect_config              0x00016cbc   Section        0  drv_lcdc.o(i.drv_lcdc_edge_dect_config)
    i.drv_lcdc_edge_enh_config               0x00016cf8   Section        0  drv_lcdc.o(i.drv_lcdc_edge_enh_config)
    i.drv_lcdc_enable_shadow_reg             0x00016d5c   Section        0  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    i.drv_lcdc_endianness_config             0x00016d80   Section        0  drv_lcdc.o(i.drv_lcdc_endianness_config)
    i.drv_lcdc_fc_config                     0x00016d9c   Section        0  drv_lcdc.o(i.drv_lcdc_fc_config)
    i.drv_lcdc_fldc_config                   0x00016dbc   Section        0  drv_lcdc.o(i.drv_lcdc_fldc_config)
    i.drv_lcdc_function_disable              0x00016de0   Section        0  drv_lcdc.o(i.drv_lcdc_function_disable)
    i.drv_lcdc_function_enable               0x00016e04   Section        0  drv_lcdc.o(i.drv_lcdc_function_enable)
    i.drv_lcdc_set_int                       0x00016e28   Section        0  drv_lcdc.o(i.drv_lcdc_set_int)
    i.drv_lcdc_set_prefetch                  0x00016e64   Section        0  drv_lcdc.o(i.drv_lcdc_set_prefetch)
    i.drv_lcdc_set_tear_line                 0x00016e80   Section        0  drv_lcdc.o(i.drv_lcdc_set_tear_line)
    i.drv_lcdc_stop_display                  0x00016e9c   Section        0  drv_lcdc.o(i.drv_lcdc_stop_display)
    i.drv_lcdc_vid_hw_start                  0x00016eac   Section        0  drv_lcdc.o(i.drv_lcdc_vid_hw_start)
    i.drv_lcdc_vintp_mode_config             0x00016ee8   Section        0  drv_lcdc.o(i.drv_lcdc_vintp_mode_config)
    i.drv_memc_clear_status                  0x00016f00   Section        0  drv_memc.o(i.drv_memc_clear_status)
    i.drv_memc_enable_irq                    0x00016f14   Section        0  drv_memc.o(i.drv_memc_enable_irq)
    i.drv_memc_gen_a_tear_signal             0x00016f54   Section        0  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    i.drv_memc_get_status                    0x00016f64   Section        0  drv_memc.o(i.drv_memc_get_status)
    i.drv_memc_get_tear_mode                 0x00016f7c   Section        0  drv_memc.o(i.drv_memc_get_tear_mode)
    i.drv_memc_rate_transfer_sel             0x00016f8c   Section        0  drv_memc.o(i.drv_memc_rate_transfer_sel)
    i.drv_memc_sel_vsync                     0x00016fa8   Section        0  drv_memc.o(i.drv_memc_sel_vsync)
    i.drv_memc_set_active_height             0x00016fbc   Section        0  drv_memc.o(i.drv_memc_set_active_height)
    i.drv_memc_set_circ_mode_enable          0x00016fd4   Section        0  drv_memc.o(i.drv_memc_set_circ_mode_enable)
    i.drv_memc_set_data_mode                 0x00016ff0   Section        0  drv_memc.o(i.drv_memc_set_data_mode)
    i.drv_memc_set_double_buffer             0x00017004   Section        0  drv_memc.o(i.drv_memc_set_double_buffer)
    i.drv_memc_set_frame_drop_select         0x0001701c   Section        0  drv_memc.o(i.drv_memc_set_frame_drop_select)
    i.drv_memc_set_fs_en_conditions          0x00017038   Section        0  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    i.drv_memc_set_lcdc_st_conditions        0x00017050   Section        0  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    i.drv_memc_set_ltpo_mode                 0x0001706c   Section        0  drv_memc.o(i.drv_memc_set_ltpo_mode)
    i.drv_memc_set_ltpo_pu_thres             0x0001708c   Section        0  drv_memc.o(i.drv_memc_set_ltpo_pu_thres)
    i.drv_memc_set_tear_mode                 0x000170a4   Section        0  drv_memc.o(i.drv_memc_set_tear_mode)
    i.drv_memc_set_tear_waveform             0x000170b8   Section        0  drv_memc.o(i.drv_memc_set_tear_waveform)
    i.drv_memc_set_vidc_sync_cnt             0x000170e4   Section        0  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    i.drv_phy_test_clear                     0x000170f8   Section        0  drv_phy_common.o(i.drv_phy_test_clear)
    i.drv_phy_test_lock                      0x00017108   Section        0  drv_phy_common.o(i.drv_phy_test_lock)
    i.drv_pwr_efuse_pd                       0x00017120   Section        0  drv_pwr.o(i.drv_pwr_efuse_pd)
    i.drv_pwr_enter_deep_sleep_mode          0x00017150   Section        0  drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode)
    i.drv_pwr_enter_sleep_mode_ex            0x0001719c   Section        0  drv_pwr.o(i.drv_pwr_enter_sleep_mode_ex)
    i.drv_pwr_enter_stop_sleep_mode          0x000171d0   Section        0  drv_pwr.o(i.drv_pwr_enter_stop_sleep_mode)
    i.drv_pwr_exit_sleep_mode                0x00017268   Section        0  drv_pwr.o(i.drv_pwr_exit_sleep_mode)
    i.drv_pwr_get_power_ready_st             0x00017290   Section        0  drv_pwr.o(i.drv_pwr_get_power_ready_st)
    i.drv_pwr_set_breath_screen_power_sel    0x000172a0   Section        0  drv_pwr.o(i.drv_pwr_set_breath_screen_power_sel)
    i.drv_pwr_set_digit_power_sel            0x000172c8   Section        0  drv_pwr.o(i.drv_pwr_set_digit_power_sel)
    i.drv_pwr_set_pll_clk                    0x000172f0   Section        0  drv_pwr.o(i.drv_pwr_set_pll_clk)
    i.drv_pwr_set_wakeup_type                0x00017324   Section        0  drv_pwr.o(i.drv_pwr_set_wakeup_type)
    i.drv_pwr_write_lock                     0x00017350   Section        0  drv_pwr.o(i.drv_pwr_write_lock)
    i.drv_rxbr_clear_pkt_buffer              0x00017370   Section        0  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    i.drv_rxbr_clear_status0                 0x00017380   Section        0  drv_rxbr.o(i.drv_rxbr_clear_status0)
    i.drv_rxbr_enable_irq                    0x0001738c   Section        0  drv_rxbr.o(i.drv_rxbr_enable_irq)
    i.drv_rxbr_frame_drop_cfg                0x000173e8   Section        0  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    i.drv_rxbr_get_int_source                0x00017404   Section        0  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    drv_rxbr_get_int_source                  0x00017405   Thumb Code    20  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    i.drv_rxbr_get_status0                   0x0001741c   Section        0  hal_internal_dcs.o(i.drv_rxbr_get_status0)
    drv_rxbr_get_status0                     0x0001741d   Thumb Code    20  hal_internal_dcs.o(i.drv_rxbr_get_status0)
    i.drv_rxbr_hline_rcv1_cfg                0x00017434   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg)
    i.drv_rxbr_hline_rcv_cfg                 0x00017448   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    i.drv_rxbr_register_irq1_callback        0x00017458   Section        0  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    i.drv_rxbr_set_ack_pkt_header            0x00017464   Section        0  drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header)
    i.drv_rxbr_set_color_format              0x0001747c   Section        0  drv_rxbr.o(i.drv_rxbr_set_color_format)
    i.drv_rxbr_set_filter_regs               0x00017498   Section        0  drv_rxbr.o(i.drv_rxbr_set_filter_regs)
    i.drv_rxbr_set_inten                     0x000174bc   Section        0  drv_rxbr.o(i.drv_rxbr_set_inten)
    i.drv_rxbr_set_ltpo_drop_th              0x000174d8   Section        0  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    i.drv_rxbr_set_usr_cfg                   0x000174f0   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    i.drv_rxbr_set_usr_col                   0x00017530   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    i.drv_rxbr_set_usr_row                   0x00017540   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    i.drv_se_init                            0x00017550   Section        0  drv_se.o(i.drv_se_init)
    i.drv_se_set_dsc                         0x000175c8   Section        0  drv_se.o(i.drv_se_set_dsc)
    i.drv_se_set_lcdc                        0x0001769c   Section        0  drv_se.o(i.drv_se_set_lcdc)
    i.drv_se_set_memc                        0x00017724   Section        0  drv_se.o(i.drv_se_set_memc)
    i.drv_se_set_rxbr                        0x0001778c   Section        0  drv_se.o(i.drv_se_set_rxbr)
    i.drv_se_set_vidc                        0x0001785c   Section        0  drv_se.o(i.drv_se_set_vidc)
    i.drv_se_start_rx                        0x00017908   Section        0  drv_se.o(i.drv_se_start_rx)
    i.drv_swire_enable                       0x0001791c   Section        0  drv_swire.o(i.drv_swire_enable)
    i.drv_swire_get_pulse_count              0x00017938   Section        0  drv_swire.o(i.drv_swire_get_pulse_count)
    i.drv_swire_register_callback            0x00017944   Section        0  drv_swire.o(i.drv_swire_register_callback)
    i.drv_swire_set_bit_time                 0x00017950   Section        0  drv_swire.o(i.drv_swire_set_bit_time)
    i.drv_swire_set_int                      0x00017968   Section        0  drv_swire.o(i.drv_swire_set_int)
    i.drv_swire_set_power_down               0x000179b0   Section        0  drv_swire.o(i.drv_swire_set_power_down)
    i.drv_swire_set_pulse_count              0x000179cc   Section        0  drv_swire.o(i.drv_swire_set_pulse_count)
    i.drv_swire_set_trig_mode                0x000179d8   Section        0  drv_swire.o(i.drv_swire_set_trig_mode)
    i.drv_sys_cfg_clear_all_int              0x000179f4   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    i.drv_sys_cfg_clear_pending              0x00017a00   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    i.drv_sys_cfg_sel_ap_rst_trig            0x00017a28   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig)
    i.drv_sys_cfg_sel_gpio_group             0x00017a4c   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group)
    i.drv_sys_cfg_sel_int_trig               0x00017a70   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig)
    i.drv_sys_cfg_sel_swire_timer            0x00017a94   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_swire_timer)
    i.drv_sys_cfg_set_int                    0x00017aac   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    i.drv_timer_clear_status_flags           0x00017ad0   Section        0  drv_timer.o(i.drv_timer_clear_status_flags)
    drv_timer_clear_status_flags             0x00017ad1   Thumb Code    26  drv_timer.o(i.drv_timer_clear_status_flags)
    i.drv_timer_enable                       0x00017aea   Section        0  drv_timer.o(i.drv_timer_enable)
    i.drv_timer_get_instance                 0x00017b0c   Section        0  drv_timer.o(i.drv_timer_get_instance)
    i.drv_timer_handle_interrupt             0x00017b1c   Section        0  drv_timer.o(i.drv_timer_handle_interrupt)
    drv_timer_handle_interrupt               0x00017b1d   Thumb Code    54  drv_timer.o(i.drv_timer_handle_interrupt)
    i.drv_timer_set_compare_val              0x00017b58   Section        0  drv_timer.o(i.drv_timer_set_compare_val)
    i.drv_timer_set_int                      0x00017b98   Section        0  drv_timer.o(i.drv_timer_set_int)
    i.drv_timer_set_prescaler                0x00017be0   Section        0  drv_timer.o(i.drv_timer_set_prescaler)
    i.drv_timer_set_repeat                   0x00017c08   Section        0  drv_timer.o(i.drv_timer_set_repeat)
    i.drv_tx_phy_test_enter                  0x00017c18   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    i.drv_tx_phy_test_exit                   0x00017c38   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    i.drv_tx_phy_test_write_code             0x00017c58   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    i.drv_uart_abort_recv                    0x00017c80   Section        0  drv_uart.o(i.drv_uart_abort_recv)
    i.drv_uart_abort_send                    0x00017cb4   Section        0  drv_uart.o(i.drv_uart_abort_send)
    i.drv_uart_config_int                    0x00017ce8   Section        0  drv_uart.o(i.drv_uart_config_int)
    i.drv_uart_enable_clk                    0x00017cfc   Section        0  drv_uart.o(i.drv_uart_enable_clk)
    drv_uart_enable_clk                      0x00017cfd   Thumb Code    24  drv_uart.o(i.drv_uart_enable_clk)
    i.drv_uart_enable_int                    0x00017d14   Section        0  drv_uart.o(i.drv_uart_enable_int)
    i.drv_uart_get_instance                  0x00017d70   Section        0  drv_uart.o(i.drv_uart_get_instance)
    i.drv_uart_init                          0x00017d98   Section        0  drv_uart.o(i.drv_uart_init)
    i.drv_uart_int_trans_handle              0x00017e68   Section        0  drv_uart.o(i.drv_uart_int_trans_handle)
    drv_uart_int_trans_handle                0x00017e69   Thumb Code    54  drv_uart.o(i.drv_uart_int_trans_handle)
    i.drv_uart_reset_rx_fifo                 0x00017ea4   Section        0  drv_uart.o(i.drv_uart_reset_rx_fifo)
    i.drv_uart_reset_tx_fifo                 0x00017ec0   Section        0  drv_uart.o(i.drv_uart_reset_tx_fifo)
    i.drv_uart_send_blocking                 0x00017edc   Section        0  drv_uart.o(i.drv_uart_send_blocking)
    i.drv_uart_set_baud_rate                 0x00017ef6   Section        0  drv_uart.o(i.drv_uart_set_baud_rate)
    i.drv_uart_trans_create_handle           0x00017f4c   Section        0  drv_uart.o(i.drv_uart_trans_create_handle)
    i.drv_vidc_clear_irq                     0x00017f98   Section        0  drv_vidc.o(i.drv_vidc_clear_irq)
    i.drv_vidc_enable                        0x00017fa8   Section        0  drv_vidc.o(i.drv_vidc_enable)
    i.drv_vidc_enable_irq                    0x00017fc8   Section        0  drv_vidc.o(i.drv_vidc_enable_irq)
    i.drv_vidc_get_int_source                0x00018008   Section        0  drv_vidc.o(i.drv_vidc_get_int_source)
    i.drv_vidc_get_irq_status                0x00018034   Section        0  drv_vidc.o(i.drv_vidc_get_irq_status)
    i.drv_vidc_init_module_enable            0x0001804c   Section        0  drv_vidc.o(i.drv_vidc_init_module_enable)
    i.drv_vidc_register_callback             0x00018078   Section        0  drv_vidc.o(i.drv_vidc_register_callback)
    i.drv_vidc_reset                         0x00018084   Section        0  drv_vidc.o(i.drv_vidc_reset)
    i.drv_vidc_set_circ_mode_enable          0x00018090   Section        0  drv_vidc.o(i.drv_vidc_set_circ_mode_enable)
    i.drv_vidc_set_dither_config             0x000180ac   Section        0  drv_vidc.o(i.drv_vidc_set_dither_config)
    i.drv_vidc_set_dst_parameter             0x000180e4   Section        0  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    i.drv_vidc_set_honly_hcoef0              0x00018140   Section        0  drv_vidc.o(i.drv_vidc_set_honly_hcoef0)
    i.drv_vidc_set_honly_hinitb              0x0001814c   Section        0  drv_vidc.o(i.drv_vidc_set_honly_hinitb)
    i.drv_vidc_set_honly_hinitr              0x00018178   Section        0  drv_vidc.o(i.drv_vidc_set_honly_hinitr)
    i.drv_vidc_set_irqen                     0x000181a8   Section        0  drv_vidc.o(i.drv_vidc_set_irqen)
    i.drv_vidc_set_mirror                    0x000181c4   Section        0  drv_vidc.o(i.drv_vidc_set_mirror)
    i.drv_vidc_set_pentile_swap              0x000181d8   Section        0  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    i.drv_vidc_set_pu_ctrl                   0x000181f4   Section        0  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    i.drv_vidc_set_rotation                  0x00018200   Section        0  drv_vidc.o(i.drv_vidc_set_rotation)
    i.drv_vidc_set_scld_hcoef0               0x00018218   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    i.drv_vidc_set_scld_hcoef1               0x00018224   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    i.drv_vidc_set_scld_step                 0x00018230   Section        0  drv_vidc.o(i.drv_vidc_set_scld_step)
    i.drv_vidc_set_scld_vcoef0               0x00018244   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    i.drv_vidc_set_scld_vcoef1               0x00018250   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    i.drv_vidc_set_src_parameter             0x0001825c   Section        0  drv_vidc.o(i.drv_vidc_set_src_parameter)
    i.drv_vidc_set_vintp_config              0x0001827c   Section        0  drv_vidc.o(i.drv_vidc_set_vintp_config)
    i.fputc                                  0x000182b4   Section        0  tau_log.o(i.fputc)
    i.google_p6a_demo                        0x000182e8   Section        0  p6a_demo.o(i.google_p6a_demo)
    i.ha_intl_fb_check_pu_size               0x00018348   Section        0  hal_internal_fb.o(i.ha_intl_fb_check_pu_size)
    ha_intl_fb_check_pu_size                 0x00018349   Thumb Code    58  hal_internal_fb.o(i.ha_intl_fb_check_pu_size)
    i.hal_dsi_rx_ctrl_create_handle          0x00018388   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    i.hal_dsi_rx_ctrl_dcs_async_handler      0x000183c8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler)
    i.hal_dsi_rx_ctrl_deinit                 0x00018408   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit)
    i.hal_dsi_rx_ctrl_get_max_ret_size       0x0001849c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size)
    i.hal_dsi_rx_ctrl_init                   0x000184bc   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    i.hal_dsi_rx_ctrl_init_clk               0x00018568   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    hal_dsi_rx_ctrl_init_clk                 0x00018569   Thumb Code   222  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    i.hal_dsi_rx_ctrl_init_dsi_rx            0x00018668   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    hal_dsi_rx_ctrl_init_dsi_rx              0x00018669   Thumb Code   232  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    i.hal_dsi_rx_ctrl_init_memc              0x00018770   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    hal_dsi_rx_ctrl_init_memc                0x00018771   Thumb Code   294  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    i.hal_dsi_rx_ctrl_init_rxbr              0x0001889c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    hal_dsi_rx_ctrl_init_rxbr                0x0001889d   Thumb Code   314  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    i.hal_dsi_rx_ctrl_init_vidc              0x000189e4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    hal_dsi_rx_ctrl_init_vidc                0x000189e5   Thumb Code   624  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    i.hal_dsi_rx_ctrl_pre_init_pps           0x00018c64   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    i.hal_dsi_rx_ctrl_send_ack_cmd           0x00018c9c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd)
    i.hal_dsi_rx_ctrl_set_ipi_cfg            0x00018d8c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    hal_dsi_rx_ctrl_set_ipi_cfg              0x00018d8d   Thumb Code    48  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    i.hal_dsi_rx_ctrl_start                  0x00018dbc   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    i.hal_dsi_rx_ctrl_stop                   0x00018dec   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop)
    i.hal_dsi_rx_ctrl_toggle_resolution      0x00018e1c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    i.hal_dsi_tx_cmd_mode_cal_timing         0x00018e3c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing)
    hal_dsi_tx_cmd_mode_cal_timing           0x00018e3d   Thumb Code   510  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing)
    i.hal_dsi_tx_ctrl_create_handle          0x000190bc   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    i.hal_dsi_tx_ctrl_deinit                 0x000190f4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit)
    i.hal_dsi_tx_ctrl_gen_a_tear_signal      0x00019168   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal)
    i.hal_dsi_tx_ctrl_init                   0x0001918c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    i.hal_dsi_tx_ctrl_init_clk               0x00019208   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    hal_dsi_tx_ctrl_init_clk                 0x00019209   Thumb Code    12  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    i.hal_dsi_tx_ctrl_set_overwrite_rgb      0x00019218   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    i.hal_dsi_tx_ctrl_set_tear_mode          0x00019220   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode)
    i.hal_dsi_tx_ctrl_start                  0x0001922c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    i.hal_dsi_tx_ctrl_stop                   0x000192bc   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop)
    i.hal_dsi_tx_ctrl_write_cmd              0x000192f4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    i.hal_dsi_tx_init_cfg                    0x000193c4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg)
    hal_dsi_tx_init_cfg                      0x000193c5   Thumb Code   250  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg)
    i.hal_dsi_tx_init_dpi_timing             0x000194c8   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing)
    hal_dsi_tx_init_dpi_timing               0x000194c9   Thumb Code    58  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing)
    i.hal_dsi_tx_init_phy_cfg                0x0001950c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    hal_dsi_tx_init_phy_cfg                  0x0001950d   Thumb Code    22  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    i.hal_dsi_tx_init_timing                 0x00019522   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing)
    hal_dsi_tx_init_timing                   0x00019523   Thumb Code    82  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing)
    i.hal_dsi_tx_init_vid_timing             0x00019574   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing)
    hal_dsi_tx_init_vid_timing               0x00019575   Thumb Code    70  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing)
    i.hal_dsi_tx_send_cmd                    0x000195c8   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    hal_dsi_tx_send_cmd                      0x000195c9   Thumb Code    58  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    i.hal_dsi_tx_timing_info_update          0x00019608   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update)
    hal_dsi_tx_timing_info_update            0x00019609   Thumb Code   142  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update)
    i.hal_dsi_tx_vid_mode_cal_timing         0x0001969c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing)
    hal_dsi_tx_vid_mode_cal_timing           0x0001969d   Thumb Code   766  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing)
    i.hal_gpio_config_pad                    0x000199ac   Section        0  hal_gpio.o(i.hal_gpio_config_pad)
    i.hal_gpio_ctrl_eint                     0x000199e8   Section        0  hal_gpio.o(i.hal_gpio_ctrl_eint)
    i.hal_gpio_init_eint                     0x00019a00   Section        0  hal_gpio.o(i.hal_gpio_init_eint)
    i.hal_gpio_init_input                    0x00019a40   Section        0  hal_gpio.o(i.hal_gpio_init_input)
    i.hal_gpio_init_output                   0x00019a56   Section        0  hal_gpio.o(i.hal_gpio_init_output)
    i.hal_gpio_reg_eint_cb                   0x00019a74   Section        0  hal_gpio.o(i.hal_gpio_reg_eint_cb)
    i.hal_gpio_set_ap_reset_int              0x00019a90   Section        0  hal_gpio.o(i.hal_gpio_set_ap_reset_int)
    i.hal_gpio_set_mode                      0x00019ae0   Section        0  hal_gpio.o(i.hal_gpio_set_mode)
    i.hal_gpio_set_output_data               0x00019b40   Section        0  hal_gpio.o(i.hal_gpio_set_output_data)
    i.hal_internal_sync_get_hight_performan_mode 0x00019b48   Section        0  hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode)
    i.hal_internal_sync_input_resolution_change 0x00019b58   Section        0  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    i.hal_internal_sync_register_lcdc_cb     0x00019d0c   Section        0  hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb)
    i.hal_internal_vsync_deinit              0x00019d18   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    i.hal_internal_vsync_get_rx_state        0x00019d38   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state)
    i.hal_internal_vsync_get_sync_line       0x00019d44   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    i.hal_internal_vsync_get_tx_state        0x00019d58   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    i.hal_internal_vsync_init_rx             0x00019d64   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    i.hal_internal_vsync_init_tx             0x00019e4c   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    i.hal_internal_vsync_set_rx_state        0x00019f14   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    i.hal_internal_vsync_set_tear_mode       0x00019f34   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    i.hal_internal_vsync_set_tx_state        0x0001a120   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    i.hal_intl_dcs_init_sw_fltr              0x0001a178   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr)
    i.hal_intl_dcs_rx_get_dcs_packet_data    0x0001a1e4   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data)
    hal_intl_dcs_rx_get_dcs_packet_data      0x0001a1e5   Thumb Code   782  hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data)
    i.hal_intl_dcs_rx_receive_packet         0x0001a614   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet)
    hal_intl_dcs_rx_receive_packet           0x0001a615   Thumb Code   122  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet)
    i.hal_intl_dcs_rx_receive_pps            0x0001a69c   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps)
    hal_intl_dcs_rx_receive_pps              0x0001a69d   Thumb Code   266  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps)
    i.hal_intl_dcs_set_auto_hw_filter        0x0001a810   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter)
    i.hal_intl_dcs_sw_filter_handle          0x0001a89c   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle)
    hal_intl_dcs_sw_filter_handle            0x0001a89d   Thumb Code    36  hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle)
    i.hal_intl_fb_cal_fb_info                0x0001a8c8   Section        0  hal_internal_fb.o(i.hal_intl_fb_cal_fb_info)
    i.hal_intl_fb_check_bandwidth            0x0001abe0   Section        0  hal_internal_fb.o(i.hal_intl_fb_check_bandwidth)
    hal_intl_fb_check_bandwidth              0x0001abe1   Thumb Code    92  hal_internal_fb.o(i.hal_intl_fb_check_bandwidth)
    i.hal_intl_fb_edge_resize                0x0001ac44   Section        0  hal_internal_fb.o(i.hal_intl_fb_edge_resize)
    hal_intl_fb_edge_resize                  0x0001ac45   Thumb Code   214  hal_internal_fb.o(i.hal_intl_fb_edge_resize)
    i.hal_intl_fb_flow_control_adapter       0x0001ad20   Section        0  hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter)
    hal_intl_fb_flow_control_adapter         0x0001ad21   Thumb Code   110  hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter)
    i.hal_intl_fb_get_memc_flow_mode         0x0001ad94   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode)
    i.hal_intl_fb_get_rx_fb_info             0x0001ada0   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info)
    i.hal_intl_fb_get_tx_fb_info             0x0001adb0   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info)
    i.hal_intl_fb_get_user_flow              0x0001adc0   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_user_flow)
    i.hal_intl_svs_deinit_rx                 0x0001adcc   Section        0  hal_internal_svs.o(i.hal_intl_svs_deinit_rx)
    i.hal_intl_svs_deinit_tx                 0x0001adf4   Section        0  hal_internal_svs.o(i.hal_intl_svs_deinit_tx)
    i.hal_intl_svs_handle                    0x0001ae04   Section        0  hal_internal_svs.o(i.hal_intl_svs_handle)
    i.hal_intl_svs_init_rx                   0x0001ae28   Section        0  hal_internal_svs.o(i.hal_intl_svs_init_rx)
    i.hal_intl_svs_init_tx                   0x0001aea8   Section        0  hal_internal_svs.o(i.hal_intl_svs_init_tx)
    i.hal_intl_svs_set_rx_vtt                0x0001aebc   Section        0  hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt)
    i.hal_intl_svs_update_rxbr_clk           0x0001aec8   Section        0  hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk)
    i.hal_lcdc_displayproc_config            0x0001af10   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config)
    i.hal_lcdc_init_cfg                      0x0001af80   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    hal_lcdc_init_cfg                        0x0001af81   Thumb Code    62  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    i.hal_lcdc_init_clk                      0x0001afbe   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    hal_lcdc_init_clk                        0x0001afbf   Thumb Code   112  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    i.hal_lcdc_postproc_config               0x0001b030   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config)
    i.hal_lcdc_start                         0x0001b158   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_start)
    hal_lcdc_start                           0x0001b159   Thumb Code    36  hal_dsi_tx_ctrl.o(i.hal_lcdc_start)
    i.hal_lcdc_timinggen_config              0x0001b17c   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config)
    hal_lcdc_timinggen_config                0x0001b17d   Thumb Code    60  hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config)
    i.hal_lcdc_upscaler_config               0x0001b1b8   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config)
    i.hal_nonshadow_func_update              0x0001b298   Section        0  hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update)
    i.hal_pwr_enter_deep_sleep_mode          0x0001b354   Section        0  hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode)
    i.hal_pwr_enter_normal_sleep_mode        0x0001b37e   Section        0  hal_pwr.o(i.hal_pwr_enter_normal_sleep_mode)
    i.hal_pwr_enter_stop_sleep_mode          0x0001b388   Section        0  hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode)
    i.hal_pwr_exit_sleep_mode                0x0001b3ec   Section        0  hal_pwr.o(i.hal_pwr_exit_sleep_mode)
    i.hal_pwr_get_vcc_power_ready            0x0001b3f6   Section        0  hal_pwr.o(i.hal_pwr_get_vcc_power_ready)
    i.hal_pwr_set_main_power                 0x0001b3fe   Section        0  hal_pwr.o(i.hal_pwr_set_main_power)
    i.hal_pwr_set_sleep_mode_power           0x0001b406   Section        0  hal_pwr.o(i.hal_pwr_set_sleep_mode_power)
    i.hal_pwr_set_stop_sleep_wakeup_pin      0x0001b410   Section        0  hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin)
    i.hal_swire_deinit                       0x0001b474   Section        0  hal_swire.o(i.hal_swire_deinit)
    i.hal_swire_enable                       0x0001b4b4   Section        0  hal_swire.o(i.hal_swire_enable)
    i.hal_swire_init                         0x0001b510   Section        0  hal_swire.o(i.hal_swire_init)
    i.hal_swire_set_pulse                    0x0001b568   Section        0  hal_swire.o(i.hal_swire_set_pulse)
    i.hal_swire_set_timer                    0x0001b58c   Section        0  hal_swire.o(i.hal_swire_set_timer)
    i.hal_system_init                        0x0001b5cc   Section        0  hal_system.o(i.hal_system_init)
    i.hal_system_updata_sysclk               0x0001b6b0   Section        0  hal_system.o(i.hal_system_updata_sysclk)
    i.hal_timer_deinit                       0x0001b700   Section        0  hal_timer.o(i.hal_timer_deinit)
    i.hal_timer_init                         0x0001b730   Section        0  hal_timer.o(i.hal_timer_init)
    i.hal_timer_set_repeat                   0x0001b74c   Section        0  hal_timer.o(i.hal_timer_set_repeat)
    i.hal_tx_frame_rate_adjust               0x0001b754   Section        0  hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust)
    hal_tx_frame_rate_adjust                 0x0001b755   Thumb Code    44  hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust)
    i.hal_uart_init                          0x0001b784   Section        0  hal_uart.o(i.hal_uart_init)
    i.hal_uart_send_blocking                 0x0001b818   Section        0  hal_uart.o(i.hal_uart_send_blocking)
    i.hal_vsync_func_update                  0x0001b834   Section        0  hal_dsi_tx_ctrl.o(i.hal_vsync_func_update)
    i.hal_vsync_reset_lcdc_scaler            0x0001b84c   Section        0  hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler)
    i.main                                   0x0001b92c   Section        0  main.o(i.main)
    i.pps_update_handle                      0x0001b96c   Section        0  p6a_demo.o(i.pps_update_handle)
    pps_update_handle                        0x0001b96d   Thumb Code   110  p6a_demo.o(i.pps_update_handle)
    i.rxbr_irq1_callback                     0x0001b9e8   Section        0  hal_internal_vsync.o(i.rxbr_irq1_callback)
    rxbr_irq1_callback                       0x0001b9e9   Thumb Code   478  hal_internal_vsync.o(i.rxbr_irq1_callback)
    i.soft_double_buffer_update              0x0001bccc   Section        0  hal_internal_vsync.o(i.soft_double_buffer_update)
    soft_double_buffer_update                0x0001bccd   Thumb Code    56  hal_internal_vsync.o(i.soft_double_buffer_update)
    i.soft_gen_te                            0x0001bd10   Section        0  hal_internal_vsync.o(i.soft_gen_te)
    soft_gen_te                              0x0001bd11   Thumb Code    86  hal_internal_vsync.o(i.soft_gen_te)
    i.soft_gen_te_double_buffer              0x0001bd7c   Section        0  hal_internal_vsync.o(i.soft_gen_te_double_buffer)
    soft_gen_te_double_buffer                0x0001bd7d   Thumb Code   202  hal_internal_vsync.o(i.soft_gen_te_double_buffer)
    i.soft_pro_motion_init                   0x0001be5c   Section        0  hal_internal_vsync.o(i.soft_pro_motion_init)
    soft_pro_motion_init                     0x0001be5d   Thumb Code    46  hal_internal_vsync.o(i.soft_pro_motion_init)
    i.soft_tear_adjust_line                  0x0001be94   Section        0  hal_internal_vsync.o(i.soft_tear_adjust_line)
    soft_tear_adjust_line                    0x0001be95   Thumb Code    26  hal_internal_vsync.o(i.soft_tear_adjust_line)
    i.stop_sleep_cb                          0x0001beb8   Section        0  hal_pwr.o(i.stop_sleep_cb)
    stop_sleep_cb                            0x0001beb9   Thumb Code    18  hal_pwr.o(i.stop_sleep_cb)
    i.svs_direct_mode_setting                0x0001bed0   Section        0  hal_internal_svs.o(i.svs_direct_mode_setting)
    svs_direct_mode_setting                  0x0001bed1   Thumb Code   154  hal_internal_svs.o(i.svs_direct_mode_setting)
    i.svs_get_rel_intv                       0x0001bf7c   Section        0  hal_internal_svs.o(i.svs_get_rel_intv)
    svs_get_rel_intv                         0x0001bf7d   Thumb Code    20  hal_internal_svs.o(i.svs_get_rel_intv)
    i.svs_sync_handle                        0x0001bf98   Section        0  hal_internal_svs.o(i.svs_sync_handle)
    svs_sync_handle                          0x0001bf99   Thumb Code   158  hal_internal_svs.o(i.svs_sync_handle)
    i.svs_wait_fr_stab                       0x0001c048   Section        0  hal_internal_svs.o(i.svs_wait_fr_stab)
    svs_wait_fr_stab                         0x0001c049   Thumb Code   148  hal_internal_svs.o(i.svs_wait_fr_stab)
    i.svs_wait_start                         0x0001c114   Section        0  hal_internal_svs.o(i.svs_wait_start)
    svs_wait_start                           0x0001c115   Thumb Code   250  hal_internal_svs.o(i.svs_wait_start)
    i.tau_log_init                           0x0001c220   Section        0  tau_log.o(i.tau_log_init)
    i.tau_log_printf                         0x0001c254   Section        0  tau_log.o(i.tau_log_printf)
    i.tau_log_push_log                       0x0001c2d8   Section        0  tau_log.o(i.tau_log_push_log)
    i.vidc_callback                          0x0001c350   Section        0  hal_internal_vsync.o(i.vidc_callback)
    vidc_callback                            0x0001c351   Thumb Code   150  hal_internal_vsync.o(i.vidc_callback)
    i.vpre_err_reset                         0x0001c404   Section        0  hal_internal_vsync.o(i.vpre_err_reset)
    vpre_err_reset                           0x0001c405   Thumb Code   254  hal_internal_vsync.o(i.vpre_err_reset)
    .constdata                               0x0001c51c   Section       88  p6a_demo.o(.constdata)
    g_cus_rx_dcs_execute_table               0x0001c51c   Data          72  p6a_demo.o(.constdata)
    .constdata                               0x0001c574   Section       40  hal_dsi_rx_ctrl.o(.constdata)
    .constdata                               0x0001c59c   Section       28  hal_dsi_tx_ctrl.o(.constdata)
    .constdata                               0x0001c5b8   Section      182  hal_gpio.o(.constdata)
    s_gpio_map                               0x0001c5b8   Data         104  hal_gpio.o(.constdata)
    s_gpio_perf                              0x0001c620   Data          78  hal_gpio.o(.constdata)
    .constdata                               0x0001c670   Section       48  hal_uart.o(.constdata)
    .constdata                               0x0001c6a0   Section       16  drv_uart.o(.constdata)
    .conststring                             0x0001c6b0   Section       66  hal_dsi_rx_ctrl.o(.conststring)
    .conststring                             0x0001c6f4   Section      144  hal_internal_vsync.o(.conststring)
    .conststring                             0x0001c784   Section       70  hal_internal_dcs.o(.conststring)
    .data                                    0x00070000   Section      159  p6a_demo.o(.data)
    g_rx_ctrl_handle                         0x00070000   Data           4  p6a_demo.o(.data)
    g_tx_ctrl_handle                         0x00070004   Data           4  p6a_demo.o(.data)
    panel_display_done                       0x00070008   Data           1  p6a_demo.o(.data)
    sg_system_resume                         0x00070009   Data           1  p6a_demo.o(.data)
    sg_system_suspend                        0x0007000a   Data           1  p6a_demo.o(.data)
    sg_exit_idle_mode_flag                   0x0007000b   Data           1  p6a_demo.o(.data)
    g_resolution_change                      0x0007000c   Data           1  p6a_demo.o(.data)
    pps_renew_flag                           0x00070010   Data           4  p6a_demo.o(.data)
    pwr_rst_flag                             0x00070014   Data           4  p6a_demo.o(.data)
    reg53_E8_fg                              0x0007009e   Data           1  p6a_demo.o(.data)
    .data                                    0x000700a0   Section       48  hal_dsi_rx_ctrl.o(.data)
    g_hw_auto_filter                         0x000700a0   Data           1  hal_dsi_rx_ctrl.o(.data)
    g_crc_check_enable                       0x000700a1   Data           1  hal_dsi_rx_ctrl.o(.data)
    g_esc_clk                                0x000700a4   Data           4  hal_dsi_rx_ctrl.o(.data)
    g_before_draw_col                        0x000700a8   Data           4  hal_dsi_rx_ctrl.o(.data)
    g_before_draw_page                       0x000700ac   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_step                                 0x000700b0   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_cmd_filter                           0x000700b4   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_x                                    0x000700b8   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_y                                    0x000700bc   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_value                                0x000700c0   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_x                                    0x000700c4   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_y                                    0x000700c8   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_value                                0x000700cc   Data           4  hal_dsi_rx_ctrl.o(.data)
    .data                                    0x000700d0   Section       92  hal_dsi_tx_ctrl.o(.data)
    sg_bta_vsync_flag                        0x000700d0   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_vsync_flag                            0x000700d1   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_enter_sleep_cmd                       0x000700d2   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_fldc_cg_mode                          0x000700d3   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_scl_fir                        0x000700d4   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_honly_bypass_fir                      0x000700d5   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_bcs                            0x000700d6   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_enhc                           0x000700d7   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_edge_dect                      0x000700d8   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_edge_enh                       0x000700d9   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_dith                           0x000700da   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_dith_judge                            0x000700db   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_endianness                            0x000700dc   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_test_pattern_en                       0x000700dd   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_dith_judge_thr                        0x000700e0   Data           4  hal_dsi_tx_ctrl.o(.data)
    sg_ccm_para                              0x000700e4   Data          36  hal_dsi_tx_ctrl.o(.data)
    sg_honly_para                            0x00070108   Data          36  hal_dsi_tx_ctrl.o(.data)
    .data                                    0x0007012c   Section        2  hal_swire.o(.data)
    sg_swire_timer                           0x0007012c   Data           1  hal_swire.o(.data)
    sg_swire_repeat                          0x0007012d   Data           1  hal_swire.o(.data)
    .data                                    0x00070130   Section        8  hal_pwr.o(.data)
    sg_wake_up_io                            0x00070130   Data           1  hal_pwr.o(.data)
    sg_stop_sleep_wakeup_int                 0x00070134   Data           4  hal_pwr.o(.data)
    .data                                    0x00070138   Section        1  tau_log.o(.data)
    g_log_port                               0x00070138   Data           1  tau_log.o(.data)
    .data                                    0x0007013c   Section       24  hal_uart.o(.data)
    sg_dma_callback                          0x0007014c   Data           4  hal_uart.o(.data)
    sg_user_data                             0x00070150   Data           4  hal_uart.o(.data)
    .data                                    0x00070154   Section       16  hal_internal_vsync.o(.data)
    s_te_refine_mode                         0x00070154   Data           1  hal_internal_vsync.o(.data)
    .data                                    0x00070164   Section       36  hal_internal_dcs.o(.data)
    g_imm_packet                             0x00070164   Data          24  hal_internal_dcs.o(.data)
    g_cus_rx_write_cmd_handle                0x0007017c   Data          12  hal_internal_dcs.o(.data)
    .data                                    0x00070188   Section       12  drv_common.o(.data)
    s_my_tick                                0x00070188   Data           4  drv_common.o(.data)
    .data                                    0x00070194   Section        1  drv_common.o(.data)
    .data                                    0x00070198   Section        4  drv_gpio.o(.data)
    g_ap_reset_cb                            0x00070198   Data           4  drv_gpio.o(.data)
    .data                                    0x0007019c   Section        4  drv_swire.o(.data)
    sg_drv_swire_cb                          0x0007019c   Data           4  drv_swire.o(.data)
    .data                                    0x000701a0   Section       80  drv_timer.o(.data)
    sg_timer_info                            0x000701a0   Data          80  drv_timer.o(.data)
    .data                                    0x000701f0   Section        4  drv_se.o(.data)
    chip_info                                0x000701f0   Data           4  drv_se.o(.data)
    .data                                    0x000701f4   Section        1  drv_dsi_rx.o(.data)
    sg_rx_drv_level                          0x000701f4   Data           1  drv_dsi_rx.o(.data)
    .data                                    0x000701f8   Section        8  drv_rxbr.o(.data)
    .data                                    0x00070200   Section        4  drv_vidc.o(.data)
    .data                                    0x00070204   Section      400  drv_dma.o(.data)
    sg_dma_handle                            0x00070204   Data         256  drv_dma.o(.data)
    .data                                    0x00070394   Section        4  stdout.o(.data)
    .bss                                     0x00070398   Section      208  hal_dsi_rx_ctrl.o(.bss)
    g_rx_ctrl_handle                         0x00070398   Data         208  hal_dsi_rx_ctrl.o(.bss)
    .bss                                     0x00070468   Section      184  hal_dsi_tx_ctrl.o(.bss)
    g_tx_ctrl_handle                         0x00070468   Data          92  hal_dsi_tx_ctrl.o(.bss)
    sg_dsi_tx_param                          0x000704c4   Data          92  hal_dsi_tx_ctrl.o(.bss)
    .bss                                     0x00070520   Section      256  tau_log.o(.bss)
    g_log_buf                                0x00070520   Data         256  tau_log.o(.bss)
    .bss                                     0x00070620   Section       68  hal_internal_vsync.o(.bss)
    .bss                                     0x00070664   Section     2048  hal_internal_dcs.o(.bss)
    .bss                                     0x00070e64   Section      255  hal_internal_dcs.o(.bss)
    g_imm_buffer                             0x00070e64   Data         255  hal_internal_dcs.o(.bss)
    .bss                                     0x00070f64   Section       68  hal_internal_fb.o(.bss)
    .bss                                     0x00070fa8   Section       68  hal_internal_svs.o(.bss)
    sg_sys_handler                           0x00070fa8   Data          68  hal_internal_svs.o(.bss)
    .bss                                     0x00070fec   Section       64  drv_gpio.o(.bss)
    s_gpio_cb                                0x00070fec   Data          64  drv_gpio.o(.bss)
    .bss                                     0x0007102c   Section     4204  dcs_packet_fifo.o(.bss)
    .bss                                     0x00072098   Section       16  drv_dma.o(.bss)
    sg_dma_int_list                          0x00072098   Data          16  drv_dma.o(.bss)
    .bss                                     0x000720a8   Section       96  drv_uart.o(.bss)
    sg_uart_userdata                         0x000720a8   Data          96  drv_uart.o(.bss)
    STACK                                    0x00072108   Section     4096  startup_armcm0.o(STACK)

    Global Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    BuildAttributes$$THM_ISAv3M$S$PE$A:L22$X:L11$S22$IEEE1$IW$USESV6$~STKCKD$USESV7$~SHL$OTIME$ROPI$IEEEJ$EBA8$MICROLIB$REQ8$PRES8$EABIv2 0x00000000   Number         0  anon$$obj.o ABSOLUTE
    __ARM_use_no_argv                        0x00000000   Number         0  main.o ABSOLUTE
    _printf_a                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_c                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_charcount                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_d                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_e                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_f                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_flags                            0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_dec                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_hex                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_g                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_i                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_int_dec                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_l                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ll                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lld                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lli                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llo                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llu                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llx                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_dec                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_hex                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_oct                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ls                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_mbtowc                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_n                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_o                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_p                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_percent                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_pre_padding                      0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_return_value                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_s                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_sizespec                         0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_str                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_signed                  0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_unsigned                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_u                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wctomb                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_widthprec                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_x                                0x00000000   Number         0  stubs.o ABSOLUTE
    __cpp_initialize__aeabi_                  - Undefined Weak Reference
    __cxa_finalize                            - Undefined Weak Reference
    _clock_init                               - Undefined Weak Reference
    _microlib_exit                            - Undefined Weak Reference
    __Vectors_Size                           0x000000c0   Number         0  startup_armcm0.o ABSOLUTE
    __Vectors                                0x00010000   Data           4  startup_armcm0.o(RESET)
    __Vectors_End                            0x000100c0   Data           0  startup_armcm0.o(RESET)
    __main                                   0x000100c1   Thumb Code     0  entry.o(.ARM.Collect$$$$00000000)
    _main_stk                                0x000100c1   Thumb Code     0  entry2.o(.ARM.Collect$$$$00000001)
    _main_scatterload                        0x000100c5   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    __main_after_scatterload                 0x000100c9   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    _main_clock                              0x000100c9   Thumb Code     0  entry7b.o(.ARM.Collect$$$$00000008)
    _main_cpp_init                           0x000100c9   Thumb Code     0  entry8b.o(.ARM.Collect$$$$0000000A)
    _main_init                               0x000100c9   Thumb Code     0  entry9a.o(.ARM.Collect$$$$0000000B)
    __rt_final_cpp                           0x000100d1   Thumb Code     0  entry10a.o(.ARM.Collect$$$$0000000D)
    __rt_final_exit                          0x000100d1   Thumb Code     0  entry11a.o(.ARM.Collect$$$$0000000F)
    Reset_Handler                            0x000100d5   Thumb Code    28  startup_armcm0.o(.text)
    NMI_Handler                              0x000100f1   Thumb Code     2  startup_armcm0.o(.text)
    SVC_Handler                              0x000100f5   Thumb Code     2  startup_armcm0.o(.text)
    PendSV_Handler                           0x000100f7   Thumb Code     2  startup_armcm0.o(.text)
    FLSCTRL_IRQn_Handler                     0x00010107   Thumb Code     2  startup_armcm0.o(.text)
    WDG_IRQn_Handler                         0x00010113   Thumb Code     2  startup_armcm0.o(.text)
    I2C0_IRQn_Handler                        0x00010117   Thumb Code     2  startup_armcm0.o(.text)
    I2C1_IRQn_Handler                        0x00010119   Thumb Code     2  startup_armcm0.o(.text)
    SPIS_IRQn_Handler                        0x0001011b   Thumb Code     2  startup_armcm0.o(.text)
    SPIM_IRQn_Handler                        0x0001011d   Thumb Code     2  startup_armcm0.o(.text)
    I2C2_IRQn_Handler                        0x00010121   Thumb Code     2  startup_armcm0.o(.text)
    OTP_IRQn_Handler                         0x00010123   Thumb Code     2  startup_armcm0.o(.text)
    PVD_IRQn_Handler                         0x00010127   Thumb Code     2  startup_armcm0.o(.text)
    __aeabi_uidiv                            0x0001014d   Thumb Code     0  uidiv.o(.text)
    __aeabi_uidivmod                         0x0001014d   Thumb Code    44  uidiv.o(.text)
    __aeabi_idiv                             0x00010179   Thumb Code     0  idiv.o(.text)
    __aeabi_idivmod                          0x00010179   Thumb Code    40  idiv.o(.text)
    __aeabi_memcpy                           0x000101a1   Thumb Code    36  memcpya.o(.text)
    __aeabi_memcpy4                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memcpy8                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memset                           0x000101c5   Thumb Code    14  memseta.o(.text)
    __aeabi_memset4                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memset8                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr                           0x000101d3   Thumb Code     4  memseta.o(.text)
    __aeabi_memclr4                          0x000101d3   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr8                          0x000101d3   Thumb Code     0  memseta.o(.text)
    _memset$wrapper                          0x000101d7   Thumb Code    18  memseta.o(.text)
    strlen                                   0x000101e9   Thumb Code    14  strlen.o(.text)
    memcmp                                   0x000101f7   Thumb Code    26  memcmp.o(.text)
    __aeabi_fadd                             0x00010211   Thumb Code   162  fadd.o(.text)
    __aeabi_fsub                             0x000102b3   Thumb Code     8  fadd.o(.text)
    __aeabi_frsub                            0x000102bb   Thumb Code     8  fadd.o(.text)
    __aeabi_fmul                             0x000102c3   Thumb Code   122  fmul.o(.text)
    __aeabi_fdiv                             0x0001033d   Thumb Code   124  fdiv.o(.text)
    __ARM_scalbnf                            0x000103b9   Thumb Code    24  fscalb.o(.text)
    scalbnf                                  0x000103b9   Thumb Code     0  fscalb.o(.text)
    __aeabi_dadd                             0x000103d1   Thumb Code   328  dadd.o(.text)
    __aeabi_dsub                             0x00010519   Thumb Code    12  dadd.o(.text)
    __aeabi_drsub                            0x00010525   Thumb Code    12  dadd.o(.text)
    __aeabi_dmul                             0x00010535   Thumb Code   202  dmul.o(.text)
    __aeabi_ui2f                             0x00010605   Thumb Code    14  ffltui.o(.text)
    __aeabi_ui2d                             0x00010615   Thumb Code    24  dfltui.o(.text)
    __aeabi_f2uiz                            0x00010631   Thumb Code    40  ffixui.o(.text)
    __aeabi_d2uiz                            0x00010659   Thumb Code    50  dfixui.o(.text)
    __aeabi_f2d                              0x00010695   Thumb Code    40  f2d.o(.text)
    __aeabi_d2f                              0x000106bd   Thumb Code    56  d2f.o(.text)
    __aeabi_cfcmpeq                          0x000106f5   Thumb Code     0  cfcmple.o(.text)
    __aeabi_cfcmple                          0x000106f5   Thumb Code    20  cfcmple.o(.text)
    __aeabi_cfrcmple                         0x00010709   Thumb Code    20  cfrcmple.o(.text)
    __aeabi_uldivmod                         0x0001071d   Thumb Code    96  uldiv.o(.text)
    __aeabi_llsl                             0x0001077d   Thumb Code    32  llshl.o(.text)
    _ll_shift_l                              0x0001077d   Thumb Code     0  llshl.o(.text)
    __aeabi_llsr                             0x0001079d   Thumb Code    34  llushr.o(.text)
    _ll_ushift_r                             0x0001079d   Thumb Code     0  llushr.o(.text)
    __aeabi_lasr                             0x000107bf   Thumb Code    38  llsshr.o(.text)
    _ll_sshift_r                             0x000107bf   Thumb Code     0  llsshr.o(.text)
    __I$use$fp                               0x000107e5   Thumb Code     0  iusefp.o(.text)
    _float_round                             0x000107e5   Thumb Code    16  fepilogue.o(.text)
    _float_epilogue                          0x000107f5   Thumb Code   114  fepilogue.o(.text)
    _double_round                            0x00010867   Thumb Code    26  depilogue.o(.text)
    _double_epilogue                         0x00010881   Thumb Code   164  depilogue.o(.text)
    __aeabi_ddiv                             0x00010925   Thumb Code   234  ddiv.o(.text)
    __aeabi_d2ulz                            0x00010a15   Thumb Code    54  dfixul.o(.text)
    __aeabi_cdrcmple                         0x00010a55   Thumb Code    38  cdrcmple.o(.text)
    __scatterload                            0x00010a7d   Thumb Code    28  init.o(.text)
    __scatterload_rt2                        0x00010a7d   Thumb Code     0  init.o(.text)
    __decompress                             0x00010aa1   Thumb Code     0  __dczerorl2.o(.text)
    __decompress1                            0x00010aa1   Thumb Code    86  __dczerorl2.o(.text)
    AP_NRESET_IRQn_Handler                   0x00010af9   Thumb Code    22  drv_gpio.o(i.AP_NRESET_IRQn_Handler)
    DMA_IRQn_Handler                         0x00010b15   Thumb Code    78  drv_dma.o(i.DMA_IRQn_Handler)
    EXTI_INT0_IRQn_Handler                   0x00010b71   Thumb Code    10  drv_gpio.o(i.EXTI_INT0_IRQn_Handler)
    EXTI_INT1_IRQn_Handler                   0x00010b7b   Thumb Code    10  drv_gpio.o(i.EXTI_INT1_IRQn_Handler)
    EXTI_INT2_IRQn_Handler                   0x00010b85   Thumb Code    10  drv_gpio.o(i.EXTI_INT2_IRQn_Handler)
    EXTI_INT3_IRQn_Handler                   0x00010b8f   Thumb Code    10  drv_gpio.o(i.EXTI_INT3_IRQn_Handler)
    EXTI_INT4_IRQn_Handler                   0x00010b99   Thumb Code    10  drv_gpio.o(i.EXTI_INT4_IRQn_Handler)
    EXTI_INT5_IRQn_Handler                   0x00010ba3   Thumb Code    10  drv_gpio.o(i.EXTI_INT5_IRQn_Handler)
    EXTI_INT6_IRQn_Handler                   0x00010bad   Thumb Code    10  drv_gpio.o(i.EXTI_INT6_IRQn_Handler)
    EXTI_INT7_IRQn_Handler                   0x00010bb7   Thumb Code    10  drv_gpio.o(i.EXTI_INT7_IRQn_Handler)
    HardFault_Handler                        0x00010bc1   Thumb Code    14  drv_common.o(i.HardFault_Handler)
    LCDC_IRQn_Handler                        0x00010c09   Thumb Code   118  hal_internal_vsync.o(i.LCDC_IRQn_Handler)
    MEMC_IRQn_Handler                        0x00010d09   Thumb Code   154  drv_memc.o(i.MEMC_IRQn_Handler)
    MIPI_TX_IRQn_Handler                     0x00010da5   Thumb Code    70  drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler)
    SWIRE_IRQn_Handler                       0x00010e5d   Thumb Code    38  drv_swire.o(i.SWIRE_IRQn_Handler)
    SysTick_Handler                          0x00010e8d   Thumb Code    20  drv_common.o(i.SysTick_Handler)
    TIMER0_IRQn_Handler                      0x00010ea5   Thumb Code    10  drv_timer.o(i.TIMER0_IRQn_Handler)
    TIMER1_IRQn_Handler                      0x00010eaf   Thumb Code    10  drv_timer.o(i.TIMER1_IRQn_Handler)
    TIMER2_IRQn_Handler                      0x00010eb9   Thumb Code    10  drv_timer.o(i.TIMER2_IRQn_Handler)
    TIMER3_IRQn_Handler                      0x00010ec3   Thumb Code    10  drv_timer.o(i.TIMER3_IRQn_Handler)
    VIDC_IRQn_Handler                        0x00010ecd   Thumb Code    22  drv_vidc.o(i.VIDC_IRQn_Handler)
    VPRE1_IRQn_Handler                       0x00010ee9   Thumb Code    22  drv_rxbr.o(i.VPRE1_IRQn_Handler)
    VPRE_IRQn_Handler                        0x00010f05   Thumb Code   104  hal_internal_dcs.o(i.VPRE_IRQn_Handler)
    __0printf                                0x00010f71   Thumb Code    24  printfa.o(i.__0printf)
    __1printf                                0x00010f71   Thumb Code     0  printfa.o(i.__0printf)
    __2printf                                0x00010f71   Thumb Code     0  printfa.o(i.__0printf)
    __c89printf                              0x00010f71   Thumb Code     0  printfa.o(i.__0printf)
    printf                                   0x00010f71   Thumb Code     0  printfa.o(i.__0printf)
    __0vsprintf                              0x00010f91   Thumb Code    30  printfa.o(i.__0vsprintf)
    __1vsprintf                              0x00010f91   Thumb Code     0  printfa.o(i.__0vsprintf)
    __2vsprintf                              0x00010f91   Thumb Code     0  printfa.o(i.__0vsprintf)
    __c89vsprintf                            0x00010f91   Thumb Code     0  printfa.o(i.__0vsprintf)
    vsprintf                                 0x00010f91   Thumb Code     0  printfa.o(i.__0vsprintf)
    __ARM_clz                                0x00010fb5   Thumb Code    46  depilogue.o(i.__ARM_clz)
    __ARM_common_switch8                     0x00010fe3   Thumb Code    26  hal_dsi_rx_ctrl.o(i.__ARM_common_switch8)
    __scatterload_null                       0x00010ffd   Thumb Code     2  handlers.o(i.__scatterload_null)
    s_RAM_CK                                 0x00011000   Data          28  drv_common.o(.ARM.__at_0x11000)
    g_tau_log                                0x0001101c   Data          16  tau_log.o(.ARM.__at_0x1101C)
    sg_pq_para                               0x0001102c   Data          22  hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C)
    MIPI_RX_IRQn_Handler                     0x00011045   Thumb Code   354  drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler)
    UART_IRQn_Handler                        0x000113a9   Thumb Code   364  drv_uart.o(i.UART_IRQn_Handler)
    __scatterload_copy                       0x00011561   Thumb Code    14  handlers.o(i.__scatterload_copy)
    __scatterload_zeroinit                   0x0001156f   Thumb Code    14  handlers.o(i.__scatterload_zeroinit)
    app_display_init                         0x0001222d   Thumb Code    44  p6a_demo.o(i.app_display_init)
    app_gpio_init                            0x00012259   Thumb Code    22  p6a_demo.o(i.app_gpio_init)
    board_Init                               0x00015a39   Thumb Code    20  board.o(i.board_Init)
    ceil                                     0x00015a51   Thumb Code   180  ceil.o(i.ceil)
    dcs_packet_fifo_alloc                    0x00015bcd   Thumb Code    80  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    dcs_packet_fifo_init                     0x00015c25   Thumb Code    18  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    dcs_packet_free_fifo_header              0x00015c3d   Thumb Code    60  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    dcs_packet_get_fifo_header               0x00015c81   Thumb Code    26  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    delayMs                                  0x00015ca5   Thumb Code    24  tau_delay.o(i.delayMs)
    delayUs                                  0x00015cbd   Thumb Code    40  tau_delay.o(i.delayUs)
    drv_common_system_init                   0x00015ce9   Thumb Code     8  drv_common.o(i.drv_common_system_init)
    drv_crgu_enable_clock                    0x00015cf1   Thumb Code    54  drv_crgu.o(i.drv_crgu_enable_clock)
    drv_crgu_get_rxbr_clk                    0x00015d2d   Thumb Code    70  drv_crgu.o(i.drv_crgu_get_rxbr_clk)
    drv_crgu_reset_modules                   0x00015d95   Thumb Code    10  drv_crgu.o(i.drv_crgu_reset_modules)
    drv_crgu_set_ahb_clk                     0x00015da5   Thumb Code    34  drv_crgu.o(i.drv_crgu_set_ahb_clk)
    drv_crgu_set_clock_div                   0x00015dcd   Thumb Code    12  drv_crgu.o(i.drv_crgu_set_clock_div)
    drv_crgu_set_dpi_clk                     0x00015ddd   Thumb Code    54  drv_crgu.o(i.drv_crgu_set_dpi_clk)
    drv_crgu_set_dsc_clk                     0x00015e19   Thumb Code    52  drv_crgu.o(i.drv_crgu_set_dsc_clk)
    drv_crgu_set_fb_clk                      0x00015e51   Thumb Code    34  drv_crgu.o(i.drv_crgu_set_fb_clk)
    drv_crgu_set_lcdc_clk                    0x00015e79   Thumb Code    36  drv_crgu.o(i.drv_crgu_set_lcdc_clk)
    drv_crgu_set_reset                       0x00015ea1   Thumb Code    20  drv_crgu.o(i.drv_crgu_set_reset)
    drv_crgu_set_rxbr_clk                    0x00015eb9   Thumb Code    34  drv_crgu.o(i.drv_crgu_set_rxbr_clk)
    drv_crgu_set_vidc_clk                    0x00015ee1   Thumb Code    36  drv_crgu.o(i.drv_crgu_set_vidc_clk)
    drv_dma_clear_status                     0x00015f09   Thumb Code    20  drv_dma.o(i.drv_dma_clear_status)
    drv_dsc_dec_disable                      0x00015f35   Thumb Code    20  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    drv_dsc_dec_enable                       0x00015f51   Thumb Code    44  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    drv_dsc_dec_get_nslc                     0x00015f89   Thumb Code    22  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    drv_dsc_dec_set_irqen                    0x00015fa9   Thumb Code    24  drv_dsc_dec.o(i.drv_dsc_dec_set_irqen)
    drv_dsi_rx_calc_ipi_tx_delay             0x00015fc5   Thumb Code   252  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    drv_dsi_rx_enable_irq                    0x000160d1   Thumb Code    58  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    drv_dsi_rx_get_compression_en            0x0001617d   Thumb Code    10  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    drv_dsi_rx_get_ddi_crc_en                0x0001618d   Thumb Code    10  drv_dsi_rx.o(i.drv_dsi_rx_get_ddi_crc_en)
    drv_dsi_rx_get_max_ret_size              0x0001619d   Thumb Code     8  drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size)
    drv_dsi_rx_power_up                      0x000161a9   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    drv_dsi_rx_set_check_crc                 0x000161c1   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc)
    drv_dsi_rx_set_ctrl_cfg                  0x000161dd   Thumb Code    32  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    drv_dsi_rx_set_ddi_cfg                   0x00016201   Thumb Code    10  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    drv_dsi_rx_set_ddi_crc_en                0x00016211   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_crc_en)
    drv_dsi_rx_set_inten                     0x0001622d   Thumb Code     8  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    drv_dsi_rx_set_ipi_cfg                   0x00016239   Thumb Code    12  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    drv_dsi_rx_set_ipi_ycbcr_frmt            0x00016249   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_ycbcr_frmt)
    drv_dsi_rx_set_lane_swap                 0x00016265   Thumb Code    16  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    drv_dsi_rx_set_resp_cnt                  0x00016279   Thumb Code    32  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    drv_dsi_rx_set_tear_resp_en              0x0001629d   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_tear_resp_en)
    drv_dsi_rx_set_up_phy                    0x000162b9   Thumb Code   224  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    drv_dsi_rx_shut_down                     0x000163b9   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    drv_dsi_tx_command_header                0x000163d1   Thumb Code    18  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    drv_dsi_tx_command_mode_cfg              0x000163e9   Thumb Code    82  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    drv_dsi_tx_command_put_payload           0x00016441   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    drv_dsi_tx_config_eotp                   0x0001644d   Thumb Code    26  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    drv_dsi_tx_config_int                    0x0001646d   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    drv_dsi_tx_dpi_lpcmd_time                0x00016479   Thumb Code    10  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    drv_dsi_tx_dpi_mode                      0x00016489   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    drv_dsi_tx_dpi_polarity                  0x00016499   Thumb Code    32  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    drv_dsi_tx_edpi_cmd_size                 0x000164bd   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    drv_dsi_tx_get_cmd_status                0x000164c9   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    drv_dsi_tx_mode                          0x000164d5   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    drv_dsi_tx_phy_clock_lane_auto_lp        0x000164e1   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    drv_dsi_tx_phy_clock_lane_req_hs         0x000164fd   Thumb Code    26  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    drv_dsi_tx_phy_lane_mode                 0x0001651d   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    drv_dsi_tx_phy_status_ready              0x0001652d   Thumb Code   100  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    drv_dsi_tx_phy_status_stopstate          0x00016595   Thumb Code    62  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    drv_dsi_tx_phy_test_setup                0x000165d9   Thumb Code   314  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    drv_dsi_tx_phy_time_cfg                  0x00016729   Thumb Code    28  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    drv_dsi_tx_powerup                       0x00016749   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    drv_dsi_tx_response_mode                 0x00016755   Thumb Code    30  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    drv_dsi_tx_set_bta_ack                   0x00016779   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    drv_dsi_tx_set_esc_div                   0x00016795   Thumb Code    14  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    drv_dsi_tx_set_int                       0x000167a9   Thumb Code    58  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    drv_dsi_tx_set_time_out_div              0x000167e9   Thumb Code    18  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    drv_dsi_tx_set_video_chunk               0x00016801   Thumb Code    14  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    drv_dsi_tx_set_video_timing              0x00016815   Thumb Code    30  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    drv_dsi_tx_shutdown                      0x00016839   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    drv_dsi_tx_timeout_cfg                   0x00016845   Thumb Code    38  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    drv_dsi_tx_video_mode_cfg                0x00016871   Thumb Code   226  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    drv_efuse_enter_inactive                 0x00016959   Thumb Code    54  drv_efuse.o(i.drv_efuse_enter_inactive)
    drv_efuse_int_enable                     0x0001698f   Thumb Code    12  drv_efuse.o(i.drv_efuse_int_enable)
    drv_efuse_read                           0x0001699b   Thumb Code    58  drv_efuse.o(i.drv_efuse_read)
    drv_efuse_read_req                       0x000169d5   Thumb Code    24  drv_efuse.o(i.drv_efuse_read_req)
    drv_gpio_register_ap_reset_callback      0x00016a11   Thumb Code     6  drv_gpio.o(i.drv_gpio_register_ap_reset_callback)
    drv_gpio_register_callback               0x00016a1d   Thumb Code    14  drv_gpio.o(i.drv_gpio_register_callback)
    drv_gpio_set_int                         0x00016a31   Thumb Code    62  drv_gpio.o(i.drv_gpio_set_int)
    drv_gpio_set_ioe                         0x00016a75   Thumb Code    26  drv_gpio.o(i.drv_gpio_set_ioe)
    drv_gpio_set_mode                        0x00016a95   Thumb Code    16  drv_gpio.o(i.drv_gpio_set_mode)
    drv_lcdc_bcsa_config                     0x00016ac9   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_bcsa_config)
    drv_lcdc_cfg_int_frame                   0x00016af1   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_cfg_int_frame)
    drv_lcdc_cmd_start                       0x00016b35   Thumb Code    46  drv_lcdc.o(i.drv_lcdc_cmd_start)
    drv_lcdc_config_acc_command_mode         0x00016b69   Thumb Code    14  drv_lcdc.o(i.drv_lcdc_config_acc_command_mode)
    drv_lcdc_config_int                      0x00016b7d   Thumb Code    50  drv_lcdc.o(i.drv_lcdc_config_int)
    drv_lcdc_config_int_single               0x00016bb5   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_int_single)
    drv_lcdc_config_overwrite_rgb            0x00016bdd   Thumb Code    18  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    drv_lcdc_config_src_parameter            0x00016bf5   Thumb Code    72  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    drv_lcdc_crop_hact                       0x00016c45   Thumb Code    10  drv_lcdc.o(i.drv_lcdc_crop_hact)
    drv_lcdc_ctrl_flow                       0x00016c55   Thumb Code    50  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    drv_lcdc_dith_config                     0x00016c8d   Thumb Code    40  drv_lcdc.o(i.drv_lcdc_dith_config)
    drv_lcdc_edge_dect_config                0x00016cbd   Thumb Code    50  drv_lcdc.o(i.drv_lcdc_edge_dect_config)
    drv_lcdc_edge_enh_config                 0x00016cf9   Thumb Code    86  drv_lcdc.o(i.drv_lcdc_edge_enh_config)
    drv_lcdc_enable_shadow_reg               0x00016d5d   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    drv_lcdc_endianness_config               0x00016d81   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_endianness_config)
    drv_lcdc_fc_config                       0x00016d9d   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_fc_config)
    drv_lcdc_fldc_config                     0x00016dbd   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_fldc_config)
    drv_lcdc_function_disable                0x00016de1   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_function_disable)
    drv_lcdc_function_enable                 0x00016e05   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_function_enable)
    drv_lcdc_set_int                         0x00016e29   Thumb Code    54  drv_lcdc.o(i.drv_lcdc_set_int)
    drv_lcdc_set_prefetch                    0x00016e65   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_set_prefetch)
    drv_lcdc_set_tear_line                   0x00016e81   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_set_tear_line)
    drv_lcdc_stop_display                    0x00016e9d   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_stop_display)
    drv_lcdc_vid_hw_start                    0x00016ead   Thumb Code    56  drv_lcdc.o(i.drv_lcdc_vid_hw_start)
    drv_lcdc_vintp_mode_config               0x00016ee9   Thumb Code    18  drv_lcdc.o(i.drv_lcdc_vintp_mode_config)
    drv_memc_clear_status                    0x00016f01   Thumb Code    14  drv_memc.o(i.drv_memc_clear_status)
    drv_memc_enable_irq                      0x00016f15   Thumb Code    58  drv_memc.o(i.drv_memc_enable_irq)
    drv_memc_gen_a_tear_signal               0x00016f55   Thumb Code    12  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    drv_memc_get_status                      0x00016f65   Thumb Code    20  drv_memc.o(i.drv_memc_get_status)
    drv_memc_get_tear_mode                   0x00016f7d   Thumb Code    10  drv_memc.o(i.drv_memc_get_tear_mode)
    drv_memc_rate_transfer_sel               0x00016f8d   Thumb Code    22  drv_memc.o(i.drv_memc_rate_transfer_sel)
    drv_memc_sel_vsync                       0x00016fa9   Thumb Code    16  drv_memc.o(i.drv_memc_sel_vsync)
    drv_memc_set_active_height               0x00016fbd   Thumb Code    16  drv_memc.o(i.drv_memc_set_active_height)
    drv_memc_set_circ_mode_enable            0x00016fd5   Thumb Code    24  drv_memc.o(i.drv_memc_set_circ_mode_enable)
    drv_memc_set_data_mode                   0x00016ff1   Thumb Code    14  drv_memc.o(i.drv_memc_set_data_mode)
    drv_memc_set_double_buffer               0x00017005   Thumb Code    18  drv_memc.o(i.drv_memc_set_double_buffer)
    drv_memc_set_frame_drop_select           0x0001701d   Thumb Code    24  drv_memc.o(i.drv_memc_set_frame_drop_select)
    drv_memc_set_fs_en_conditions            0x00017039   Thumb Code    18  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    drv_memc_set_lcdc_st_conditions          0x00017051   Thumb Code    20  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    drv_memc_set_ltpo_mode                   0x0001706d   Thumb Code    28  drv_memc.o(i.drv_memc_set_ltpo_mode)
    drv_memc_set_ltpo_pu_thres               0x0001708d   Thumb Code    18  drv_memc.o(i.drv_memc_set_ltpo_pu_thres)
    drv_memc_set_tear_mode                   0x000170a5   Thumb Code    16  drv_memc.o(i.drv_memc_set_tear_mode)
    drv_memc_set_tear_waveform               0x000170b9   Thumb Code    36  drv_memc.o(i.drv_memc_set_tear_waveform)
    drv_memc_set_vidc_sync_cnt               0x000170e5   Thumb Code    16  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    drv_phy_test_clear                       0x000170f9   Thumb Code    16  drv_phy_common.o(i.drv_phy_test_clear)
    drv_phy_test_lock                        0x00017109   Thumb Code    24  drv_phy_common.o(i.drv_phy_test_lock)
    drv_pwr_efuse_pd                         0x00017121   Thumb Code    36  drv_pwr.o(i.drv_pwr_efuse_pd)
    drv_pwr_enter_deep_sleep_mode            0x00017151   Thumb Code    60  drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode)
    drv_pwr_enter_sleep_mode_ex              0x0001719d   Thumb Code    34  drv_pwr.o(i.drv_pwr_enter_sleep_mode_ex)
    drv_pwr_enter_stop_sleep_mode            0x000171d1   Thumb Code   132  drv_pwr.o(i.drv_pwr_enter_stop_sleep_mode)
    drv_pwr_exit_sleep_mode                  0x00017269   Thumb Code    32  drv_pwr.o(i.drv_pwr_exit_sleep_mode)
    drv_pwr_get_power_ready_st               0x00017291   Thumb Code    10  drv_pwr.o(i.drv_pwr_get_power_ready_st)
    drv_pwr_set_breath_screen_power_sel      0x000172a1   Thumb Code    34  drv_pwr.o(i.drv_pwr_set_breath_screen_power_sel)
    drv_pwr_set_digit_power_sel              0x000172c9   Thumb Code    34  drv_pwr.o(i.drv_pwr_set_digit_power_sel)
    drv_pwr_set_pll_clk                      0x000172f1   Thumb Code    30  drv_pwr.o(i.drv_pwr_set_pll_clk)
    drv_pwr_set_wakeup_type                  0x00017325   Thumb Code    40  drv_pwr.o(i.drv_pwr_set_wakeup_type)
    drv_pwr_write_lock                       0x00017351   Thumb Code    18  drv_pwr.o(i.drv_pwr_write_lock)
    drv_rxbr_clear_pkt_buffer                0x00017371   Thumb Code    12  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    drv_rxbr_clear_status0                   0x00017381   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_clear_status0)
    drv_rxbr_enable_irq                      0x0001738d   Thumb Code    90  drv_rxbr.o(i.drv_rxbr_enable_irq)
    drv_rxbr_frame_drop_cfg                  0x000173e9   Thumb Code    18  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    drv_rxbr_hline_rcv1_cfg                  0x00017435   Thumb Code    14  drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg)
    drv_rxbr_hline_rcv_cfg                   0x00017449   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    drv_rxbr_register_irq1_callback          0x00017459   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    drv_rxbr_set_ack_pkt_header              0x00017465   Thumb Code    18  drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header)
    drv_rxbr_set_color_format                0x0001747d   Thumb Code    24  drv_rxbr.o(i.drv_rxbr_set_color_format)
    drv_rxbr_set_filter_regs                 0x00017499   Thumb Code    32  drv_rxbr.o(i.drv_rxbr_set_filter_regs)
    drv_rxbr_set_inten                       0x000174bd   Thumb Code    22  drv_rxbr.o(i.drv_rxbr_set_inten)
    drv_rxbr_set_ltpo_drop_th                0x000174d9   Thumb Code    18  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    drv_rxbr_set_usr_cfg                     0x000174f1   Thumb Code    56  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    drv_rxbr_set_usr_col                     0x00017531   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    drv_rxbr_set_usr_row                     0x00017541   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    drv_se_init                              0x00017551   Thumb Code   106  drv_se.o(i.drv_se_init)
    drv_se_set_dsc                           0x000175c9   Thumb Code   162  drv_se.o(i.drv_se_set_dsc)
    drv_se_set_lcdc                          0x0001769d   Thumb Code    88  drv_se.o(i.drv_se_set_lcdc)
    drv_se_set_memc                          0x00017725   Thumb Code    54  drv_se.o(i.drv_se_set_memc)
    drv_se_set_rxbr                          0x0001778d   Thumb Code   158  drv_se.o(i.drv_se_set_rxbr)
    drv_se_set_vidc                          0x0001785d   Thumb Code   122  drv_se.o(i.drv_se_set_vidc)
    drv_se_start_rx                          0x00017909   Thumb Code    16  drv_se.o(i.drv_se_start_rx)
    drv_swire_enable                         0x0001791d   Thumb Code    24  drv_swire.o(i.drv_swire_enable)
    drv_swire_get_pulse_count                0x00017939   Thumb Code     6  drv_swire.o(i.drv_swire_get_pulse_count)
    drv_swire_register_callback              0x00017945   Thumb Code     6  drv_swire.o(i.drv_swire_register_callback)
    drv_swire_set_bit_time                   0x00017951   Thumb Code    18  drv_swire.o(i.drv_swire_set_bit_time)
    drv_swire_set_int                        0x00017969   Thumb Code    64  drv_swire.o(i.drv_swire_set_int)
    drv_swire_set_power_down                 0x000179b1   Thumb Code    24  drv_swire.o(i.drv_swire_set_power_down)
    drv_swire_set_pulse_count                0x000179cd   Thumb Code     6  drv_swire.o(i.drv_swire_set_pulse_count)
    drv_swire_set_trig_mode                  0x000179d9   Thumb Code    24  drv_swire.o(i.drv_swire_set_trig_mode)
    drv_sys_cfg_clear_all_int                0x000179f5   Thumb Code     8  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    drv_sys_cfg_clear_pending                0x00017a01   Thumb Code    32  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    drv_sys_cfg_sel_ap_rst_trig              0x00017a29   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig)
    drv_sys_cfg_sel_gpio_group               0x00017a4d   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group)
    drv_sys_cfg_sel_int_trig                 0x00017a71   Thumb Code    32  drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig)
    drv_sys_cfg_sel_swire_timer              0x00017a95   Thumb Code    18  drv_sys_cfg.o(i.drv_sys_cfg_sel_swire_timer)
    drv_sys_cfg_set_int                      0x00017aad   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    drv_timer_enable                         0x00017aeb   Thumb Code    32  drv_timer.o(i.drv_timer_enable)
    drv_timer_get_instance                   0x00017b0d   Thumb Code    10  drv_timer.o(i.drv_timer_get_instance)
    drv_timer_set_compare_val                0x00017b59   Thumb Code    50  drv_timer.o(i.drv_timer_set_compare_val)
    drv_timer_set_int                        0x00017b99   Thumb Code    68  drv_timer.o(i.drv_timer_set_int)
    drv_timer_set_prescaler                  0x00017be1   Thumb Code    36  drv_timer.o(i.drv_timer_set_prescaler)
    drv_timer_set_repeat                     0x00017c09   Thumb Code    12  drv_timer.o(i.drv_timer_set_repeat)
    drv_tx_phy_test_enter                    0x00017c19   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    drv_tx_phy_test_exit                     0x00017c39   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    drv_tx_phy_test_write_code               0x00017c59   Thumb Code    34  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    drv_uart_abort_recv                      0x00017c81   Thumb Code    46  drv_uart.o(i.drv_uart_abort_recv)
    drv_uart_abort_send                      0x00017cb5   Thumb Code    46  drv_uart.o(i.drv_uart_abort_send)
    drv_uart_config_int                      0x00017ce9   Thumb Code    20  drv_uart.o(i.drv_uart_config_int)
    drv_uart_enable_int                      0x00017d15   Thumb Code    84  drv_uart.o(i.drv_uart_enable_int)
    drv_uart_get_instance                    0x00017d71   Thumb Code    36  drv_uart.o(i.drv_uart_get_instance)
    drv_uart_init                            0x00017d99   Thumb Code   206  drv_uart.o(i.drv_uart_init)
    drv_uart_reset_rx_fifo                   0x00017ea5   Thumb Code    28  drv_uart.o(i.drv_uart_reset_rx_fifo)
    drv_uart_reset_tx_fifo                   0x00017ec1   Thumb Code    28  drv_uart.o(i.drv_uart_reset_tx_fifo)
    drv_uart_send_blocking                   0x00017edd   Thumb Code    26  drv_uart.o(i.drv_uart_send_blocking)
    drv_uart_set_baud_rate                   0x00017ef7   Thumb Code    84  drv_uart.o(i.drv_uart_set_baud_rate)
    drv_uart_trans_create_handle             0x00017f4d   Thumb Code    72  drv_uart.o(i.drv_uart_trans_create_handle)
    drv_vidc_clear_irq                       0x00017f99   Thumb Code    10  drv_vidc.o(i.drv_vidc_clear_irq)
    drv_vidc_enable                          0x00017fa9   Thumb Code    26  drv_vidc.o(i.drv_vidc_enable)
    drv_vidc_enable_irq                      0x00017fc9   Thumb Code    58  drv_vidc.o(i.drv_vidc_enable_irq)
    drv_vidc_get_int_source                  0x00018009   Thumb Code    40  drv_vidc.o(i.drv_vidc_get_int_source)
    drv_vidc_get_irq_status                  0x00018035   Thumb Code    20  drv_vidc.o(i.drv_vidc_get_irq_status)
    drv_vidc_init_module_enable              0x0001804d   Thumb Code    36  drv_vidc.o(i.drv_vidc_init_module_enable)
    drv_vidc_register_callback               0x00018079   Thumb Code     6  drv_vidc.o(i.drv_vidc_register_callback)
    drv_vidc_reset                           0x00018085   Thumb Code     8  drv_vidc.o(i.drv_vidc_reset)
    drv_vidc_set_circ_mode_enable            0x00018091   Thumb Code    24  drv_vidc.o(i.drv_vidc_set_circ_mode_enable)
    drv_vidc_set_dither_config               0x000180ad   Thumb Code    50  drv_vidc.o(i.drv_vidc_set_dither_config)
    drv_vidc_set_dst_parameter               0x000180e5   Thumb Code    86  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    drv_vidc_set_honly_hcoef0                0x00018141   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_honly_hcoef0)
    drv_vidc_set_honly_hinitb                0x0001814d   Thumb Code    38  drv_vidc.o(i.drv_vidc_set_honly_hinitb)
    drv_vidc_set_honly_hinitr                0x00018179   Thumb Code    42  drv_vidc.o(i.drv_vidc_set_honly_hinitr)
    drv_vidc_set_irqen                       0x000181a9   Thumb Code    22  drv_vidc.o(i.drv_vidc_set_irqen)
    drv_vidc_set_mirror                      0x000181c5   Thumb Code    16  drv_vidc.o(i.drv_vidc_set_mirror)
    drv_vidc_set_pentile_swap                0x000181d9   Thumb Code    20  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    drv_vidc_set_pu_ctrl                     0x000181f5   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    drv_vidc_set_rotation                    0x00018201   Thumb Code    18  drv_vidc.o(i.drv_vidc_set_rotation)
    drv_vidc_set_scld_hcoef0                 0x00018219   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    drv_vidc_set_scld_hcoef1                 0x00018225   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    drv_vidc_set_scld_step                   0x00018231   Thumb Code    14  drv_vidc.o(i.drv_vidc_set_scld_step)
    drv_vidc_set_scld_vcoef0                 0x00018245   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    drv_vidc_set_scld_vcoef1                 0x00018251   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    drv_vidc_set_src_parameter               0x0001825d   Thumb Code    28  drv_vidc.o(i.drv_vidc_set_src_parameter)
    drv_vidc_set_vintp_config                0x0001827d   Thumb Code    52  drv_vidc.o(i.drv_vidc_set_vintp_config)
    fputc                                    0x000182b5   Thumb Code    42  tau_log.o(i.fputc)
    google_p6a_demo                          0x000182e9   Thumb Code    48  p6a_demo.o(i.google_p6a_demo)
    hal_dsi_rx_ctrl_create_handle            0x00018389   Thumb Code    60  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    hal_dsi_rx_ctrl_dcs_async_handler        0x000183c9   Thumb Code    60  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler)
    hal_dsi_rx_ctrl_deinit                   0x00018409   Thumb Code   132  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit)
    hal_dsi_rx_ctrl_get_max_ret_size         0x0001849d   Thumb Code    28  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size)
    hal_dsi_rx_ctrl_init                     0x000184bd   Thumb Code   158  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    hal_dsi_rx_ctrl_pre_init_pps             0x00018c65   Thumb Code    50  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    hal_dsi_rx_ctrl_send_ack_cmd             0x00018c9d   Thumb Code   210  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd)
    hal_dsi_rx_ctrl_start                    0x00018dbd   Thumb Code    42  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    hal_dsi_rx_ctrl_stop                     0x00018ded   Thumb Code    42  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop)
    hal_dsi_rx_ctrl_toggle_resolution        0x00018e1d   Thumb Code    28  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    hal_dsi_tx_ctrl_create_handle            0x000190bd   Thumb Code    48  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    hal_dsi_tx_ctrl_deinit                   0x000190f5   Thumb Code   102  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit)
    hal_dsi_tx_ctrl_gen_a_tear_signal        0x00019169   Thumb Code    34  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal)
    hal_dsi_tx_ctrl_init                     0x0001918d   Thumb Code   110  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    hal_dsi_tx_ctrl_set_overwrite_rgb        0x00019219   Thumb Code     8  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    hal_dsi_tx_ctrl_set_tear_mode            0x00019221   Thumb Code    10  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode)
    hal_dsi_tx_ctrl_start                    0x0001922d   Thumb Code   134  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    hal_dsi_tx_ctrl_stop                     0x000192bd   Thumb Code    52  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop)
    hal_dsi_tx_ctrl_write_cmd                0x000192f5   Thumb Code   202  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    hal_gpio_config_pad                      0x000199ad   Thumb Code    58  hal_gpio.o(i.hal_gpio_config_pad)
    hal_gpio_ctrl_eint                       0x000199e9   Thumb Code    18  hal_gpio.o(i.hal_gpio_ctrl_eint)
    hal_gpio_init_eint                       0x00019a01   Thumb Code    58  hal_gpio.o(i.hal_gpio_init_eint)
    hal_gpio_init_input                      0x00019a41   Thumb Code    22  hal_gpio.o(i.hal_gpio_init_input)
    hal_gpio_init_output                     0x00019a57   Thumb Code    28  hal_gpio.o(i.hal_gpio_init_output)
    hal_gpio_reg_eint_cb                     0x00019a75   Thumb Code    22  hal_gpio.o(i.hal_gpio_reg_eint_cb)
    hal_gpio_set_ap_reset_int                0x00019a91   Thumb Code    76  hal_gpio.o(i.hal_gpio_set_ap_reset_int)
    hal_gpio_set_mode                        0x00019ae1   Thumb Code    92  hal_gpio.o(i.hal_gpio_set_mode)
    hal_gpio_set_output_data                 0x00019b41   Thumb Code     8  hal_gpio.o(i.hal_gpio_set_output_data)
    hal_internal_sync_get_hight_performan_mode 0x00019b49   Thumb Code    10  hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode)
    hal_internal_sync_input_resolution_change 0x00019b59   Thumb Code   336  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    hal_internal_sync_register_lcdc_cb       0x00019d0d   Thumb Code     8  hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb)
    hal_internal_vsync_deinit                0x00019d19   Thumb Code    22  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    hal_internal_vsync_get_rx_state          0x00019d39   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state)
    hal_internal_vsync_get_sync_line         0x00019d45   Thumb Code    16  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    hal_internal_vsync_get_tx_state          0x00019d59   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    hal_internal_vsync_init_rx               0x00019d65   Thumb Code   206  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    hal_internal_vsync_init_tx               0x00019e4d   Thumb Code   194  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    hal_internal_vsync_set_rx_state          0x00019f15   Thumb Code    28  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    hal_internal_vsync_set_tear_mode         0x00019f35   Thumb Code   424  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    hal_internal_vsync_set_tx_state          0x0001a121   Thumb Code    78  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    hal_intl_dcs_init_sw_fltr                0x0001a179   Thumb Code    90  hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr)
    hal_intl_dcs_set_auto_hw_filter          0x0001a811   Thumb Code   130  hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter)
    hal_intl_fb_cal_fb_info                  0x0001a8c9   Thumb Code   780  hal_internal_fb.o(i.hal_intl_fb_cal_fb_info)
    hal_intl_fb_get_memc_flow_mode           0x0001ad95   Thumb Code     6  hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode)
    hal_intl_fb_get_rx_fb_info               0x0001ada1   Thumb Code    12  hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info)
    hal_intl_fb_get_tx_fb_info               0x0001adb1   Thumb Code    12  hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info)
    hal_intl_fb_get_user_flow                0x0001adc1   Thumb Code     6  hal_internal_fb.o(i.hal_intl_fb_get_user_flow)
    hal_intl_svs_deinit_rx                   0x0001adcd   Thumb Code    32  hal_internal_svs.o(i.hal_intl_svs_deinit_rx)
    hal_intl_svs_deinit_tx                   0x0001adf5   Thumb Code    10  hal_internal_svs.o(i.hal_intl_svs_deinit_tx)
    hal_intl_svs_handle                      0x0001ae05   Thumb Code    24  hal_internal_svs.o(i.hal_intl_svs_handle)
    hal_intl_svs_init_rx                     0x0001ae29   Thumb Code   120  hal_internal_svs.o(i.hal_intl_svs_init_rx)
    hal_intl_svs_init_tx                     0x0001aea9   Thumb Code    16  hal_internal_svs.o(i.hal_intl_svs_init_tx)
    hal_intl_svs_set_rx_vtt                  0x0001aebd   Thumb Code     6  hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt)
    hal_intl_svs_update_rxbr_clk             0x0001aec9   Thumb Code    52  hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk)
    hal_lcdc_displayproc_config              0x0001af11   Thumb Code    94  hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config)
    hal_lcdc_postproc_config                 0x0001b031   Thumb Code   276  hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config)
    hal_lcdc_upscaler_config                 0x0001b1b9   Thumb Code   202  hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config)
    hal_nonshadow_func_update                0x0001b299   Thumb Code   180  hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update)
    hal_pwr_enter_deep_sleep_mode            0x0001b355   Thumb Code    42  hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode)
    hal_pwr_enter_normal_sleep_mode          0x0001b37f   Thumb Code     8  hal_pwr.o(i.hal_pwr_enter_normal_sleep_mode)
    hal_pwr_enter_stop_sleep_mode            0x0001b389   Thumb Code    88  hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode)
    hal_pwr_exit_sleep_mode                  0x0001b3ed   Thumb Code    10  hal_pwr.o(i.hal_pwr_exit_sleep_mode)
    hal_pwr_get_vcc_power_ready              0x0001b3f7   Thumb Code     8  hal_pwr.o(i.hal_pwr_get_vcc_power_ready)
    hal_pwr_set_main_power                   0x0001b3ff   Thumb Code     8  hal_pwr.o(i.hal_pwr_set_main_power)
    hal_pwr_set_sleep_mode_power             0x0001b407   Thumb Code     8  hal_pwr.o(i.hal_pwr_set_sleep_mode_power)
    hal_pwr_set_stop_sleep_wakeup_pin        0x0001b411   Thumb Code    86  hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin)
    hal_swire_deinit                         0x0001b475   Thumb Code    60  hal_swire.o(i.hal_swire_deinit)
    hal_swire_enable                         0x0001b4b5   Thumb Code    86  hal_swire.o(i.hal_swire_enable)
    hal_swire_init                           0x0001b511   Thumb Code    74  hal_swire.o(i.hal_swire_init)
    hal_swire_set_pulse                      0x0001b569   Thumb Code    32  hal_swire.o(i.hal_swire_set_pulse)
    hal_swire_set_timer                      0x0001b58d   Thumb Code    60  hal_swire.o(i.hal_swire_set_timer)
    hal_system_init                          0x0001b5cd   Thumb Code   192  hal_system.o(i.hal_system_init)
    hal_system_updata_sysclk                 0x0001b6b1   Thumb Code    60  hal_system.o(i.hal_system_updata_sysclk)
    hal_timer_deinit                         0x0001b701   Thumb Code    48  hal_timer.o(i.hal_timer_deinit)
    hal_timer_init                           0x0001b731   Thumb Code    28  hal_timer.o(i.hal_timer_init)
    hal_timer_set_repeat                     0x0001b74d   Thumb Code     8  hal_timer.o(i.hal_timer_set_repeat)
    hal_uart_init                            0x0001b785   Thumb Code   134  hal_uart.o(i.hal_uart_init)
    hal_uart_send_blocking                   0x0001b819   Thumb Code    24  hal_uart.o(i.hal_uart_send_blocking)
    hal_vsync_func_update                    0x0001b835   Thumb Code    18  hal_dsi_tx_ctrl.o(i.hal_vsync_func_update)
    hal_vsync_reset_lcdc_scaler              0x0001b84d   Thumb Code   206  hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler)
    main                                     0x0001b92d   Thumb Code    32  main.o(i.main)
    tau_log_init                             0x0001c221   Thumb Code    48  tau_log.o(i.tau_log_init)
    tau_log_printf                           0x0001c255   Thumb Code   116  tau_log.o(i.tau_log_printf)
    tau_log_push_log                         0x0001c2d9   Thumb Code   118  tau_log.o(i.tau_log_push_log)
    Region$$Table$$Base                      0x0001c7cc   Number         0  anon$$obj.o(Region$$Table)
    Region$$Table$$Limit                     0x0001c7ec   Number         0  anon$$obj.o(Region$$Table)
    rd_51_val                                0x00070018   Data           2  p6a_demo.o(.data)
    rd_51_val2                               0x0007001a   Data           2  p6a_demo.o(.data)
    pps                                      0x0007001c   Data         128  p6a_demo.o(.data)
    value_51H                                0x0007009c   Data           1  p6a_demo.o(.data)
    value_51L                                0x0007009d   Data           1  p6a_demo.o(.data)
    sg_uart0_tx_handle                       0x0007013c   Data           4  hal_uart.o(.data)
    sg_uart0_rx_handle                       0x00070140   Data           4  hal_uart.o(.data)
    sg_uart1_tx_handle                       0x00070144   Data           4  hal_uart.o(.data)
    sg_uart1_rx_handle                       0x00070148   Data           4  hal_uart.o(.data)
    g_sof_gen_te_func                        0x00070158   Data           4  hal_internal_vsync.o(.data)
    hal_internal_vsync_handle_callback       0x0007015c   Data           4  hal_internal_vsync.o(.data)
    hal_internal_disp_end_handle_callback    0x00070160   Data           4  hal_internal_vsync.o(.data)
    g_systick_cb_func                        0x0007018c   Data           4  drv_common.o(.data)
    g_system_clock                           0x00070190   Data           4  drv_common.o(.data)
    g_system_delay_step                      0x00070194   Data           1  drv_common.o(.data)
    g_int_rxbr_irq0_cb_func                  0x000701f8   Data           4  drv_rxbr.o(.data)
    g_int_rxbr_irq1_cb_func                  0x000701fc   Data           4  drv_rxbr.o(.data)
    g_int_vidc_cb_func                       0x00070200   Data           4  drv_vidc.o(.data)
    dma_req_map                              0x00070304   Data         144  drv_dma.o(.data)
    __stdout                                 0x00070394   Data           4  stdout.o(.data)
    g_vsync_handle                           0x00070620   Data          40  hal_internal_vsync.o(.bss)
    sg_pro_motion_handle                     0x00070648   Data          28  hal_internal_vsync.o(.bss)
    g_dcs_execute_table                      0x00070664   Data        2048  hal_internal_dcs.o(.bss)
    g_rx_fb_info                             0x00070f64   Data          68  hal_internal_fb.o(.bss)
    g_packet_fifo                            0x0007102c   Data        4204  dcs_packet_fifo.o(.bss)
    __stack_limit                            0x00072108   Data           0  startup_armcm0.o(STACK)
    __initial_sp                             0x00073108   Data           0  startup_armcm0.o(STACK)



==============================================================================

Memory Map of the image

  Image Entry point : 0x000100c1

  Load Region LR_IROM2 (Base: 0x00010000, Size: 0x0000cb84, Max: 0x00010000, ABSOLUTE, COMPRESSED[0x0000c938])

    Execution Region ER_IROM2 (Exec base: 0x00010000, Load base: 0x00010000, Size: 0x0000c7ec, Max: 0x00010000, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00010000   0x00010000   0x000000c0   Data   RO          312    RESET               startup_armcm0.o
    0x000100c0   0x000100c0   0x00000000   Code   RO         1869  * .ARM.Collect$$$$00000000  mc_p.l(entry.o)
    0x000100c0   0x000100c0   0x00000004   Code   RO         2177    .ARM.Collect$$$$00000001  mc_p.l(entry2.o)
    0x000100c4   0x000100c4   0x00000004   Code   RO         2180    .ARM.Collect$$$$00000004  mc_p.l(entry5.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         2182    .ARM.Collect$$$$00000008  mc_p.l(entry7b.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         2184    .ARM.Collect$$$$0000000A  mc_p.l(entry8b.o)
    0x000100c8   0x000100c8   0x00000008   Code   RO         2185    .ARM.Collect$$$$0000000B  mc_p.l(entry9a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         2187    .ARM.Collect$$$$0000000D  mc_p.l(entry10a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         2189    .ARM.Collect$$$$0000000F  mc_p.l(entry11a.o)
    0x000100d0   0x000100d0   0x00000004   Code   RO         2178    .ARM.Collect$$$$00002712  mc_p.l(entry2.o)
    0x000100d4   0x000100d4   0x00000078   Code   RO          313    .text               startup_armcm0.o
    0x0001014c   0x0001014c   0x0000002c   Code   RO         1872    .text               mc_p.l(uidiv.o)
    0x00010178   0x00010178   0x00000028   Code   RO         1874    .text               mc_p.l(idiv.o)
    0x000101a0   0x000101a0   0x00000024   Code   RO         1876    .text               mc_p.l(memcpya.o)
    0x000101c4   0x000101c4   0x00000024   Code   RO         1878    .text               mc_p.l(memseta.o)
    0x000101e8   0x000101e8   0x0000000e   Code   RO         1880    .text               mc_p.l(strlen.o)
    0x000101f6   0x000101f6   0x0000001a   Code   RO         1882    .text               mc_p.l(memcmp.o)
    0x00010210   0x00010210   0x000000b2   Code   RO         2147    .text               mf_p.l(fadd.o)
    0x000102c2   0x000102c2   0x0000007a   Code   RO         2149    .text               mf_p.l(fmul.o)
    0x0001033c   0x0001033c   0x0000007c   Code   RO         2151    .text               mf_p.l(fdiv.o)
    0x000103b8   0x000103b8   0x00000018   Code   RO         2153    .text               mf_p.l(fscalb.o)
    0x000103d0   0x000103d0   0x00000164   Code   RO         2155    .text               mf_p.l(dadd.o)
    0x00010534   0x00010534   0x000000d0   Code   RO         2157    .text               mf_p.l(dmul.o)
    0x00010604   0x00010604   0x0000000e   Code   RO         2161    .text               mf_p.l(ffltui.o)
    0x00010612   0x00010612   0x00000002   PAD
    0x00010614   0x00010614   0x0000001c   Code   RO         2163    .text               mf_p.l(dfltui.o)
    0x00010630   0x00010630   0x00000028   Code   RO         2165    .text               mf_p.l(ffixui.o)
    0x00010658   0x00010658   0x0000003c   Code   RO         2167    .text               mf_p.l(dfixui.o)
    0x00010694   0x00010694   0x00000028   Code   RO         2169    .text               mf_p.l(f2d.o)
    0x000106bc   0x000106bc   0x00000038   Code   RO         2171    .text               mf_p.l(d2f.o)
    0x000106f4   0x000106f4   0x00000014   Code   RO         2173    .text               mf_p.l(cfcmple.o)
    0x00010708   0x00010708   0x00000014   Code   RO         2175    .text               mf_p.l(cfrcmple.o)
    0x0001071c   0x0001071c   0x00000060   Code   RO         2192    .text               mc_p.l(uldiv.o)
    0x0001077c   0x0001077c   0x00000020   Code   RO         2194    .text               mc_p.l(llshl.o)
    0x0001079c   0x0001079c   0x00000022   Code   RO         2196    .text               mc_p.l(llushr.o)
    0x000107be   0x000107be   0x00000026   Code   RO         2198    .text               mc_p.l(llsshr.o)
    0x000107e4   0x000107e4   0x00000000   Code   RO         2200    .text               mc_p.l(iusefp.o)
    0x000107e4   0x000107e4   0x00000082   Code   RO         2201    .text               mf_p.l(fepilogue.o)
    0x00010866   0x00010866   0x000000be   Code   RO         2203    .text               mf_p.l(depilogue.o)
    0x00010924   0x00010924   0x000000f0   Code   RO         2207    .text               mf_p.l(ddiv.o)
    0x00010a14   0x00010a14   0x00000040   Code   RO         2209    .text               mf_p.l(dfixul.o)
    0x00010a54   0x00010a54   0x00000028   Code   RO         2211    .text               mf_p.l(cdrcmple.o)
    0x00010a7c   0x00010a7c   0x00000024   Code   RO         2213    .text               mc_p.l(init.o)
    0x00010aa0   0x00010aa0   0x00000056   Code   RO         2223    .text               mc_p.l(__dczerorl2.o)
    0x00010af6   0x00010af6   0x00000002   PAD
    0x00010af8   0x00010af8   0x0000001c   Code   RO          951    i.AP_NRESET_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010b14   0x00010b14   0x0000005c   Code   RO         1718    i.DMA_IRQn_Handler  CVWL668T.lib(drv_dma.o)
    0x00010b70   0x00010b70   0x0000000a   Code   RO          952    i.EXTI_INT0_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010b7a   0x00010b7a   0x0000000a   Code   RO          953    i.EXTI_INT1_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010b84   0x00010b84   0x0000000a   Code   RO          954    i.EXTI_INT2_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010b8e   0x00010b8e   0x0000000a   Code   RO          955    i.EXTI_INT3_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010b98   0x00010b98   0x0000000a   Code   RO          956    i.EXTI_INT4_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010ba2   0x00010ba2   0x0000000a   Code   RO          957    i.EXTI_INT5_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010bac   0x00010bac   0x0000000a   Code   RO          958    i.EXTI_INT6_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010bb6   0x00010bb6   0x0000000a   Code   RO          959    i.EXTI_INT7_IRQn_Handler  CVWL668T.lib(drv_gpio.o)
    0x00010bc0   0x00010bc0   0x00000048   Code   RO          874    i.HardFault_Handler  CVWL668T.lib(drv_common.o)
    0x00010c08   0x00010c08   0x00000100   Code   RO          719    i.LCDC_IRQn_Handler  CVWL668T.lib(hal_internal_vsync.o)
    0x00010d08   0x00010d08   0x0000009a   Code   RO         1478    i.MEMC_IRQn_Handler  CVWL668T.lib(drv_memc.o)
    0x00010da2   0x00010da2   0x00000002   PAD
    0x00010da4   0x00010da4   0x000000b8   Code   RO         1284    i.MIPI_TX_IRQn_Handler  CVWL668T.lib(drv_dsi_tx.o)
    0x00010e5c   0x00010e5c   0x00000030   Code   RO         1113    i.SWIRE_IRQn_Handler  CVWL668T.lib(drv_swire.o)
    0x00010e8c   0x00010e8c   0x00000018   Code   RO          875    i.SysTick_Handler   CVWL668T.lib(drv_common.o)
    0x00010ea4   0x00010ea4   0x0000000a   Code   RO         1156    i.TIMER0_IRQn_Handler  CVWL668T.lib(drv_timer.o)
    0x00010eae   0x00010eae   0x0000000a   Code   RO         1157    i.TIMER1_IRQn_Handler  CVWL668T.lib(drv_timer.o)
    0x00010eb8   0x00010eb8   0x0000000a   Code   RO         1158    i.TIMER2_IRQn_Handler  CVWL668T.lib(drv_timer.o)
    0x00010ec2   0x00010ec2   0x0000000a   Code   RO         1159    i.TIMER3_IRQn_Handler  CVWL668T.lib(drv_timer.o)
    0x00010ecc   0x00010ecc   0x0000001c   Code   RO         1633    i.VIDC_IRQn_Handler  CVWL668T.lib(drv_vidc.o)
    0x00010ee8   0x00010ee8   0x0000001c   Code   RO         1544    i.VPRE1_IRQn_Handler  CVWL668T.lib(drv_rxbr.o)
    0x00010f04   0x00010f04   0x0000006c   Code   RO          785    i.VPRE_IRQn_Handler  CVWL668T.lib(hal_internal_dcs.o)
    0x00010f70   0x00010f70   0x00000020   Code   RO         2119    i.__0printf         mc_p.l(printfa.o)
    0x00010f90   0x00010f90   0x00000024   Code   RO         2125    i.__0vsprintf       mc_p.l(printfa.o)
    0x00010fb4   0x00010fb4   0x0000002e   Code   RO         2205    i.__ARM_clz         mf_p.l(depilogue.o)
    0x00010fe2   0x00010fe2   0x0000001a   Code   RO          407    i.__ARM_common_switch8  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00010ffc   0x00010ffc   0x00000002   Code   RO         2218    i.__scatterload_null  mc_p.l(handlers.o)
    0x00010ffe   0x00010ffe   0x00000002   PAD
    0x00011000   0x00011000   0x0000001c   Data   RO          882    .ARM.__at_0x11000   CVWL668T.lib(drv_common.o)
    0x0001101c   0x0001101c   0x00000010   Data   RO          675    .ARM.__at_0x1101C   CVWL668T.lib(tau_log.o)
    0x0001102c   0x0001102c   0x00000016   Data   RO          460    .ARM.__at_0x1102C   CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00011042   0x00011042   0x00000002   PAD
    0x00011044   0x00011044   0x00000364   Code   RO         1223    i.MIPI_RX_IRQn_Handler  CVWL668T.lib(drv_dsi_rx.o)
    0x000113a8   0x000113a8   0x00000180   Code   RO         1781    i.UART_IRQn_Handler  CVWL668T.lib(drv_uart.o)
    0x00011528   0x00011528   0x00000020   Code   RO         1545    i.__NVIC_DisableIRQ  CVWL668T.lib(drv_rxbr.o)
    0x00011548   0x00011548   0x00000018   Code   RO         1546    i.__NVIC_EnableIRQ  CVWL668T.lib(drv_rxbr.o)
    0x00011560   0x00011560   0x0000000e   Code   RO         2217    i.__scatterload_copy  mc_p.l(handlers.o)
    0x0001156e   0x0001156e   0x0000000e   Code   RO         2219    i.__scatterload_zeroinit  mc_p.l(handlers.o)
    0x0001157c   0x0001157c   0x00000174   Code   RO         2126    i._fp_digits        mc_p.l(printfa.o)
    0x000116f0   0x000116f0   0x000006ec   Code   RO         2127    i._printf_core      mc_p.l(printfa.o)
    0x00011ddc   0x00011ddc   0x00000020   Code   RO         2128    i._printf_post_padding  mc_p.l(printfa.o)
    0x00011dfc   0x00011dfc   0x0000002c   Code   RO         2129    i._printf_pre_padding  mc_p.l(printfa.o)
    0x00011e28   0x00011e28   0x0000000a   Code   RO         2131    i._sputc            mc_p.l(printfa.o)
    0x00011e32   0x00011e32   0x00000002   PAD
    0x00011e34   0x00011e34   0x00000144   Code   RO           94    i.ap_dcs_read       p6a_demo.o
    0x00011f78   0x00011f78   0x000000f0   Code   RO           95    i.ap_dcs_set_backlight  p6a_demo.o
    0x00012068   0x00012068   0x00000048   Code   RO           96    i.ap_dcs_set_display_off  p6a_demo.o
    0x000120b0   0x000120b0   0x00000044   Code   RO           97    i.ap_dcs_set_display_on  p6a_demo.o
    0x000120f4   0x000120f4   0x00000088   Code   RO           98    i.ap_dcs_set_enter_sleep_mode  p6a_demo.o
    0x0001217c   0x0001217c   0x00000040   Code   RO          100    i.ap_dcs_set_exit_sleep_mode  p6a_demo.o
    0x000121bc   0x000121bc   0x00000054   Code   RO          102    i.ap_rstn_pull_down_cb  p6a_demo.o
    0x00012210   0x00012210   0x0000001c   Code   RO          103    i.ap_rstn_pull_high_cb  p6a_demo.o
    0x0001222c   0x0001222c   0x0000002c   Code   RO          105    i.app_display_init  p6a_demo.o
    0x00012258   0x00012258   0x0000001c   Code   RO          106    i.app_gpio_init     p6a_demo.o
    0x00012274   0x00012274   0x000032ac   Code   RO          107    i.app_init_panel    p6a_demo.o
    0x00015520   0x00015520   0x0000012c   Code   RO          108    i.app_mipi_rx_init  p6a_demo.o
    0x0001564c   0x0001564c   0x0000010c   Code   RO          109    i.app_mipi_tx_init  p6a_demo.o
    0x00015758   0x00015758   0x00000070   Code   RO          110    i.app_mipi_tx_start  p6a_demo.o
    0x000157c8   0x000157c8   0x0000006c   Code   RO          111    i.app_system_process  p6a_demo.o
    0x00015834   0x00015834   0x00000044   Code   RO          112    i.app_system_resume  p6a_demo.o
    0x00015878   0x00015878   0x00000190   Code   RO          113    i.app_system_suspend  p6a_demo.o
    0x00015a08   0x00015a08   0x0000002e   Code   RO          114    i.app_tx_panel_reset  p6a_demo.o
    0x00015a36   0x00015a36   0x00000002   PAD
    0x00015a38   0x00015a38   0x00000018   Code   RO          286    i.board_Init        board.o
    0x00015a50   0x00015a50   0x000000c8   Code   RO         1866    i.ceil              m_ps.l(ceil.o)
    0x00015b18   0x00015b18   0x0000002c   Code   RO          720    i.check_mipi_rx_tx_video_info  CVWL668T.lib(hal_internal_vsync.o)
    0x00015b44   0x00015b44   0x00000088   Code   RO          786    i.check_pkt_buf_rev  CVWL668T.lib(hal_internal_dcs.o)
    0x00015bcc   0x00015bcc   0x00000058   Code   RO         1189    i.dcs_packet_fifo_alloc  CVWL668T.lib(dcs_packet_fifo.o)
    0x00015c24   0x00015c24   0x00000018   Code   RO         1190    i.dcs_packet_fifo_init  CVWL668T.lib(dcs_packet_fifo.o)
    0x00015c3c   0x00015c3c   0x00000044   Code   RO         1191    i.dcs_packet_free_fifo_header  CVWL668T.lib(dcs_packet_fifo.o)
    0x00015c80   0x00015c80   0x00000024   Code   RO         1192    i.dcs_packet_get_fifo_header  CVWL668T.lib(dcs_packet_fifo.o)
    0x00015ca4   0x00015ca4   0x00000018   Code   RO          662    i.delayMs           CVWL668T.lib(tau_delay.o)
    0x00015cbc   0x00015cbc   0x0000002c   Code   RO          663    i.delayUs           CVWL668T.lib(tau_delay.o)
    0x00015ce8   0x00015ce8   0x00000008   Code   RO          880    i.drv_common_system_init  CVWL668T.lib(drv_common.o)
    0x00015cf0   0x00015cf0   0x0000003c   Code   RO          899    i.drv_crgu_enable_clock  CVWL668T.lib(drv_crgu.o)
    0x00015d2c   0x00015d2c   0x00000068   Code   RO          902    i.drv_crgu_get_rxbr_clk  CVWL668T.lib(drv_crgu.o)
    0x00015d94   0x00015d94   0x00000010   Code   RO          905    i.drv_crgu_reset_modules  CVWL668T.lib(drv_crgu.o)
    0x00015da4   0x00015da4   0x00000028   Code   RO          906    i.drv_crgu_set_ahb_clk  CVWL668T.lib(drv_crgu.o)
    0x00015dcc   0x00015dcc   0x00000010   Code   RO          907    i.drv_crgu_set_clock_div  CVWL668T.lib(drv_crgu.o)
    0x00015ddc   0x00015ddc   0x0000003c   Code   RO          909    i.drv_crgu_set_dpi_clk  CVWL668T.lib(drv_crgu.o)
    0x00015e18   0x00015e18   0x00000038   Code   RO          910    i.drv_crgu_set_dsc_clk  CVWL668T.lib(drv_crgu.o)
    0x00015e50   0x00015e50   0x00000028   Code   RO          911    i.drv_crgu_set_fb_clk  CVWL668T.lib(drv_crgu.o)
    0x00015e78   0x00015e78   0x00000028   Code   RO          912    i.drv_crgu_set_lcdc_clk  CVWL668T.lib(drv_crgu.o)
    0x00015ea0   0x00015ea0   0x00000018   Code   RO          913    i.drv_crgu_set_reset  CVWL668T.lib(drv_crgu.o)
    0x00015eb8   0x00015eb8   0x00000028   Code   RO          914    i.drv_crgu_set_rxbr_clk  CVWL668T.lib(drv_crgu.o)
    0x00015ee0   0x00015ee0   0x00000028   Code   RO          915    i.drv_crgu_set_vidc_clk  CVWL668T.lib(drv_crgu.o)
    0x00015f08   0x00015f08   0x00000018   Code   RO         1720    i.drv_dma_clear_status  CVWL668T.lib(drv_dma.o)
    0x00015f20   0x00015f20   0x00000014   Code   RO         1726    i.drv_dma_get_int_source  CVWL668T.lib(drv_dma.o)
    0x00015f34   0x00015f34   0x0000001c   Code   RO          939    i.drv_dsc_dec_disable  CVWL668T.lib(drv_dsc_dec.o)
    0x00015f50   0x00015f50   0x00000038   Code   RO          940    i.drv_dsc_dec_enable  CVWL668T.lib(drv_dsc_dec.o)
    0x00015f88   0x00015f88   0x00000020   Code   RO          941    i.drv_dsc_dec_get_nslc  CVWL668T.lib(drv_dsc_dec.o)
    0x00015fa8   0x00015fa8   0x0000001c   Code   RO          942    i.drv_dsc_dec_set_irqen  CVWL668T.lib(drv_dsc_dec.o)
    0x00015fc4   0x00015fc4   0x0000010c   Code   RO         1224    i.drv_dsi_rx_calc_ipi_tx_delay  CVWL668T.lib(drv_dsi_rx.o)
    0x000160d0   0x000160d0   0x00000040   Code   RO         1225    i.drv_dsi_rx_enable_irq  CVWL668T.lib(drv_dsi_rx.o)
    0x00016110   0x00016110   0x00000050   Code   RO         1227    i.drv_dsi_rx_get_color_bpp  CVWL668T.lib(drv_dsi_rx.o)
    0x00016160   0x00016160   0x0000001c   Code   RO         1228    i.drv_dsi_rx_get_color_pcc  CVWL668T.lib(drv_dsi_rx.o)
    0x0001617c   0x0001617c   0x00000010   Code   RO         1229    i.drv_dsi_rx_get_compression_en  CVWL668T.lib(drv_dsi_rx.o)
    0x0001618c   0x0001618c   0x00000010   Code   RO         1230    i.drv_dsi_rx_get_ddi_crc_en  CVWL668T.lib(drv_dsi_rx.o)
    0x0001619c   0x0001619c   0x0000000c   Code   RO         1232    i.drv_dsi_rx_get_max_ret_size  CVWL668T.lib(drv_dsi_rx.o)
    0x000161a8   0x000161a8   0x00000018   Code   RO         1235    i.drv_dsi_rx_power_up  CVWL668T.lib(drv_dsi_rx.o)
    0x000161c0   0x000161c0   0x0000001c   Code   RO         1236    i.drv_dsi_rx_set_check_crc  CVWL668T.lib(drv_dsi_rx.o)
    0x000161dc   0x000161dc   0x00000024   Code   RO         1237    i.drv_dsi_rx_set_ctrl_cfg  CVWL668T.lib(drv_dsi_rx.o)
    0x00016200   0x00016200   0x00000010   Code   RO         1238    i.drv_dsi_rx_set_ddi_cfg  CVWL668T.lib(drv_dsi_rx.o)
    0x00016210   0x00016210   0x0000001c   Code   RO         1239    i.drv_dsi_rx_set_ddi_crc_en  CVWL668T.lib(drv_dsi_rx.o)
    0x0001622c   0x0001622c   0x0000000c   Code   RO         1242    i.drv_dsi_rx_set_inten  CVWL668T.lib(drv_dsi_rx.o)
    0x00016238   0x00016238   0x00000010   Code   RO         1243    i.drv_dsi_rx_set_ipi_cfg  CVWL668T.lib(drv_dsi_rx.o)
    0x00016248   0x00016248   0x0000001c   Code   RO         1245    i.drv_dsi_rx_set_ipi_ycbcr_frmt  CVWL668T.lib(drv_dsi_rx.o)
    0x00016264   0x00016264   0x00000014   Code   RO         1246    i.drv_dsi_rx_set_lane_swap  CVWL668T.lib(drv_dsi_rx.o)
    0x00016278   0x00016278   0x00000024   Code   RO         1247    i.drv_dsi_rx_set_resp_cnt  CVWL668T.lib(drv_dsi_rx.o)
    0x0001629c   0x0001629c   0x0000001c   Code   RO         1248    i.drv_dsi_rx_set_tear_resp_en  CVWL668T.lib(drv_dsi_rx.o)
    0x000162b8   0x000162b8   0x00000100   Code   RO         1249    i.drv_dsi_rx_set_up_phy  CVWL668T.lib(drv_dsi_rx.o)
    0x000163b8   0x000163b8   0x00000018   Code   RO         1250    i.drv_dsi_rx_shut_down  CVWL668T.lib(drv_dsi_rx.o)
    0x000163d0   0x000163d0   0x00000018   Code   RO         1286    i.drv_dsi_tx_command_header  CVWL668T.lib(drv_dsi_tx.o)
    0x000163e8   0x000163e8   0x00000058   Code   RO         1287    i.drv_dsi_tx_command_mode_cfg  CVWL668T.lib(drv_dsi_tx.o)
    0x00016440   0x00016440   0x0000000c   Code   RO         1288    i.drv_dsi_tx_command_put_payload  CVWL668T.lib(drv_dsi_tx.o)
    0x0001644c   0x0001644c   0x00000020   Code   RO         1289    i.drv_dsi_tx_config_eotp  CVWL668T.lib(drv_dsi_tx.o)
    0x0001646c   0x0001646c   0x0000000c   Code   RO         1290    i.drv_dsi_tx_config_int  CVWL668T.lib(drv_dsi_tx.o)
    0x00016478   0x00016478   0x00000010   Code   RO         1291    i.drv_dsi_tx_dpi_lpcmd_time  CVWL668T.lib(drv_dsi_tx.o)
    0x00016488   0x00016488   0x00000010   Code   RO         1292    i.drv_dsi_tx_dpi_mode  CVWL668T.lib(drv_dsi_tx.o)
    0x00016498   0x00016498   0x00000024   Code   RO         1293    i.drv_dsi_tx_dpi_polarity  CVWL668T.lib(drv_dsi_tx.o)
    0x000164bc   0x000164bc   0x0000000c   Code   RO         1294    i.drv_dsi_tx_edpi_cmd_size  CVWL668T.lib(drv_dsi_tx.o)
    0x000164c8   0x000164c8   0x0000000c   Code   RO         1296    i.drv_dsi_tx_get_cmd_status  CVWL668T.lib(drv_dsi_tx.o)
    0x000164d4   0x000164d4   0x0000000c   Code   RO         1298    i.drv_dsi_tx_mode   CVWL668T.lib(drv_dsi_tx.o)
    0x000164e0   0x000164e0   0x0000001c   Code   RO         1299    i.drv_dsi_tx_phy_clock_lane_auto_lp  CVWL668T.lib(drv_dsi_tx.o)
    0x000164fc   0x000164fc   0x00000020   Code   RO         1300    i.drv_dsi_tx_phy_clock_lane_req_hs  CVWL668T.lib(drv_dsi_tx.o)
    0x0001651c   0x0001651c   0x00000010   Code   RO         1302    i.drv_dsi_tx_phy_lane_mode  CVWL668T.lib(drv_dsi_tx.o)
    0x0001652c   0x0001652c   0x00000068   Code   RO         1305    i.drv_dsi_tx_phy_status_ready  CVWL668T.lib(drv_dsi_tx.o)
    0x00016594   0x00016594   0x00000044   Code   RO         1306    i.drv_dsi_tx_phy_status_stopstate  CVWL668T.lib(drv_dsi_tx.o)
    0x000165d8   0x000165d8   0x00000150   Code   RO         1308    i.drv_dsi_tx_phy_test_setup  CVWL668T.lib(drv_dsi_tx.o)
    0x00016728   0x00016728   0x00000020   Code   RO         1309    i.drv_dsi_tx_phy_time_cfg  CVWL668T.lib(drv_dsi_tx.o)
    0x00016748   0x00016748   0x0000000c   Code   RO         1313    i.drv_dsi_tx_powerup  CVWL668T.lib(drv_dsi_tx.o)
    0x00016754   0x00016754   0x00000024   Code   RO         1314    i.drv_dsi_tx_response_mode  CVWL668T.lib(drv_dsi_tx.o)
    0x00016778   0x00016778   0x0000001c   Code   RO         1317    i.drv_dsi_tx_set_bta_ack  CVWL668T.lib(drv_dsi_tx.o)
    0x00016794   0x00016794   0x00000014   Code   RO         1318    i.drv_dsi_tx_set_esc_div  CVWL668T.lib(drv_dsi_tx.o)
    0x000167a8   0x000167a8   0x00000040   Code   RO         1319    i.drv_dsi_tx_set_int  CVWL668T.lib(drv_dsi_tx.o)
    0x000167e8   0x000167e8   0x00000018   Code   RO         1320    i.drv_dsi_tx_set_time_out_div  CVWL668T.lib(drv_dsi_tx.o)
    0x00016800   0x00016800   0x00000014   Code   RO         1321    i.drv_dsi_tx_set_video_chunk  CVWL668T.lib(drv_dsi_tx.o)
    0x00016814   0x00016814   0x00000024   Code   RO         1322    i.drv_dsi_tx_set_video_timing  CVWL668T.lib(drv_dsi_tx.o)
    0x00016838   0x00016838   0x0000000c   Code   RO         1324    i.drv_dsi_tx_shutdown  CVWL668T.lib(drv_dsi_tx.o)
    0x00016844   0x00016844   0x0000002c   Code   RO         1325    i.drv_dsi_tx_timeout_cfg  CVWL668T.lib(drv_dsi_tx.o)
    0x00016870   0x00016870   0x000000e8   Code   RO         1328    i.drv_dsi_tx_video_mode_cfg  CVWL668T.lib(drv_dsi_tx.o)
    0x00016958   0x00016958   0x00000036   Code   RO         1826    i.drv_efuse_enter_inactive  CVWL668T.lib(drv_efuse.o)
    0x0001698e   0x0001698e   0x0000000c   Code   RO         1829    i.drv_efuse_int_enable  CVWL668T.lib(drv_efuse.o)
    0x0001699a   0x0001699a   0x0000003a   Code   RO         1830    i.drv_efuse_read    CVWL668T.lib(drv_efuse.o)
    0x000169d4   0x000169d4   0x00000018   Code   RO         1831    i.drv_efuse_read_req  CVWL668T.lib(drv_efuse.o)
    0x000169ec   0x000169ec   0x00000024   Code   RO          962    i.drv_gpio_handle_int  CVWL668T.lib(drv_gpio.o)
    0x00016a10   0x00016a10   0x0000000c   Code   RO          963    i.drv_gpio_register_ap_reset_callback  CVWL668T.lib(drv_gpio.o)
    0x00016a1c   0x00016a1c   0x00000014   Code   RO          964    i.drv_gpio_register_callback  CVWL668T.lib(drv_gpio.o)
    0x00016a30   0x00016a30   0x00000044   Code   RO          966    i.drv_gpio_set_int  CVWL668T.lib(drv_gpio.o)
    0x00016a74   0x00016a74   0x00000020   Code   RO          967    i.drv_gpio_set_ioe  CVWL668T.lib(drv_gpio.o)
    0x00016a94   0x00016a94   0x00000014   Code   RO          968    i.drv_gpio_set_mode  CVWL668T.lib(drv_gpio.o)
    0x00016aa8   0x00016aa8   0x00000020   Code   RO          517    i.drv_gpio_set_output_data  CVWL668T.lib(hal_gpio.o)
    0x00016ac8   0x00016ac8   0x00000028   Code   RO         1390    i.drv_lcdc_bcsa_config  CVWL668T.lib(drv_lcdc.o)
    0x00016af0   0x00016af0   0x0000002c   Code   RO         1391    i.drv_lcdc_cfg_int_frame  CVWL668T.lib(drv_lcdc.o)
    0x00016b1c   0x00016b1c   0x00000018   Code   RO         1392    i.drv_lcdc_clear_int  CVWL668T.lib(drv_lcdc.o)
    0x00016b34   0x00016b34   0x00000034   Code   RO         1394    i.drv_lcdc_cmd_start  CVWL668T.lib(drv_lcdc.o)
    0x00016b68   0x00016b68   0x00000014   Code   RO         1395    i.drv_lcdc_config_acc_command_mode  CVWL668T.lib(drv_lcdc.o)
    0x00016b7c   0x00016b7c   0x00000038   Code   RO         1396    i.drv_lcdc_config_int  CVWL668T.lib(drv_lcdc.o)
    0x00016bb4   0x00016bb4   0x00000028   Code   RO         1397    i.drv_lcdc_config_int_single  CVWL668T.lib(drv_lcdc.o)
    0x00016bdc   0x00016bdc   0x00000018   Code   RO         1398    i.drv_lcdc_config_overwrite_rgb  CVWL668T.lib(drv_lcdc.o)
    0x00016bf4   0x00016bf4   0x00000050   Code   RO         1399    i.drv_lcdc_config_src_parameter  CVWL668T.lib(drv_lcdc.o)
    0x00016c44   0x00016c44   0x00000010   Code   RO         1400    i.drv_lcdc_crop_hact  CVWL668T.lib(drv_lcdc.o)
    0x00016c54   0x00016c54   0x00000038   Code   RO         1401    i.drv_lcdc_ctrl_flow  CVWL668T.lib(drv_lcdc.o)
    0x00016c8c   0x00016c8c   0x00000030   Code   RO         1402    i.drv_lcdc_dith_config  CVWL668T.lib(drv_lcdc.o)
    0x00016cbc   0x00016cbc   0x0000003c   Code   RO         1404    i.drv_lcdc_edge_dect_config  CVWL668T.lib(drv_lcdc.o)
    0x00016cf8   0x00016cf8   0x00000064   Code   RO         1405    i.drv_lcdc_edge_enh_config  CVWL668T.lib(drv_lcdc.o)
    0x00016d5c   0x00016d5c   0x00000024   Code   RO         1406    i.drv_lcdc_enable_shadow_reg  CVWL668T.lib(drv_lcdc.o)
    0x00016d80   0x00016d80   0x0000001c   Code   RO         1407    i.drv_lcdc_endianness_config  CVWL668T.lib(drv_lcdc.o)
    0x00016d9c   0x00016d9c   0x00000020   Code   RO         1408    i.drv_lcdc_fc_config  CVWL668T.lib(drv_lcdc.o)
    0x00016dbc   0x00016dbc   0x00000024   Code   RO         1410    i.drv_lcdc_fldc_config  CVWL668T.lib(drv_lcdc.o)
    0x00016de0   0x00016de0   0x00000024   Code   RO         1411    i.drv_lcdc_function_disable  CVWL668T.lib(drv_lcdc.o)
    0x00016e04   0x00016e04   0x00000024   Code   RO         1412    i.drv_lcdc_function_enable  CVWL668T.lib(drv_lcdc.o)
    0x00016e28   0x00016e28   0x0000003c   Code   RO         1423    i.drv_lcdc_set_int  CVWL668T.lib(drv_lcdc.o)
    0x00016e64   0x00016e64   0x0000001c   Code   RO         1424    i.drv_lcdc_set_prefetch  CVWL668T.lib(drv_lcdc.o)
    0x00016e80   0x00016e80   0x0000001c   Code   RO         1425    i.drv_lcdc_set_tear_line  CVWL668T.lib(drv_lcdc.o)
    0x00016e9c   0x00016e9c   0x00000010   Code   RO         1427    i.drv_lcdc_stop_display  CVWL668T.lib(drv_lcdc.o)
    0x00016eac   0x00016eac   0x0000003c   Code   RO         1429    i.drv_lcdc_vid_hw_start  CVWL668T.lib(drv_lcdc.o)
    0x00016ee8   0x00016ee8   0x00000018   Code   RO         1431    i.drv_lcdc_vintp_mode_config  CVWL668T.lib(drv_lcdc.o)
    0x00016f00   0x00016f00   0x00000014   Code   RO         1479    i.drv_memc_clear_status  CVWL668T.lib(drv_memc.o)
    0x00016f14   0x00016f14   0x00000040   Code   RO         1480    i.drv_memc_enable_irq  CVWL668T.lib(drv_memc.o)
    0x00016f54   0x00016f54   0x00000010   Code   RO         1481    i.drv_memc_gen_a_tear_signal  CVWL668T.lib(drv_memc.o)
    0x00016f64   0x00016f64   0x00000018   Code   RO         1482    i.drv_memc_get_status  CVWL668T.lib(drv_memc.o)
    0x00016f7c   0x00016f7c   0x00000010   Code   RO         1483    i.drv_memc_get_tear_mode  CVWL668T.lib(drv_memc.o)
    0x00016f8c   0x00016f8c   0x0000001c   Code   RO         1484    i.drv_memc_rate_transfer_sel  CVWL668T.lib(drv_memc.o)
    0x00016fa8   0x00016fa8   0x00000014   Code   RO         1485    i.drv_memc_sel_vsync  CVWL668T.lib(drv_memc.o)
    0x00016fbc   0x00016fbc   0x00000018   Code   RO         1486    i.drv_memc_set_active_height  CVWL668T.lib(drv_memc.o)
    0x00016fd4   0x00016fd4   0x0000001c   Code   RO         1487    i.drv_memc_set_circ_mode_enable  CVWL668T.lib(drv_memc.o)
    0x00016ff0   0x00016ff0   0x00000014   Code   RO         1488    i.drv_memc_set_data_mode  CVWL668T.lib(drv_memc.o)
    0x00017004   0x00017004   0x00000018   Code   RO         1491    i.drv_memc_set_double_buffer  CVWL668T.lib(drv_memc.o)
    0x0001701c   0x0001701c   0x0000001c   Code   RO         1495    i.drv_memc_set_frame_drop_select  CVWL668T.lib(drv_memc.o)
    0x00017038   0x00017038   0x00000018   Code   RO         1496    i.drv_memc_set_fs_en_conditions  CVWL668T.lib(drv_memc.o)
    0x00017050   0x00017050   0x0000001c   Code   RO         1498    i.drv_memc_set_lcdc_st_conditions  CVWL668T.lib(drv_memc.o)
    0x0001706c   0x0001706c   0x00000020   Code   RO         1499    i.drv_memc_set_ltpo_mode  CVWL668T.lib(drv_memc.o)
    0x0001708c   0x0001708c   0x00000018   Code   RO         1500    i.drv_memc_set_ltpo_pu_thres  CVWL668T.lib(drv_memc.o)
    0x000170a4   0x000170a4   0x00000014   Code   RO         1504    i.drv_memc_set_tear_mode  CVWL668T.lib(drv_memc.o)
    0x000170b8   0x000170b8   0x0000002c   Code   RO         1505    i.drv_memc_set_tear_waveform  CVWL668T.lib(drv_memc.o)
    0x000170e4   0x000170e4   0x00000014   Code   RO         1507    i.drv_memc_set_vidc_sync_cnt  CVWL668T.lib(drv_memc.o)
    0x000170f8   0x000170f8   0x00000010   Code   RO         1849    i.drv_phy_test_clear  CVWL668T.lib(drv_phy_common.o)
    0x00017108   0x00017108   0x00000018   Code   RO         1850    i.drv_phy_test_lock  CVWL668T.lib(drv_phy_common.o)
    0x00017120   0x00017120   0x00000030   Code   RO          998    i.drv_pwr_efuse_pd  CVWL668T.lib(drv_pwr.o)
    0x00017150   0x00017150   0x0000004c   Code   RO         1000    i.drv_pwr_enter_deep_sleep_mode  CVWL668T.lib(drv_pwr.o)
    0x0001719c   0x0001719c   0x00000034   Code   RO         1002    i.drv_pwr_enter_sleep_mode_ex  CVWL668T.lib(drv_pwr.o)
    0x000171d0   0x000171d0   0x00000098   Code   RO         1003    i.drv_pwr_enter_stop_sleep_mode  CVWL668T.lib(drv_pwr.o)
    0x00017268   0x00017268   0x00000028   Code   RO         1004    i.drv_pwr_exit_sleep_mode  CVWL668T.lib(drv_pwr.o)
    0x00017290   0x00017290   0x00000010   Code   RO         1007    i.drv_pwr_get_power_ready_st  CVWL668T.lib(drv_pwr.o)
    0x000172a0   0x000172a0   0x00000028   Code   RO         1039    i.drv_pwr_set_breath_screen_power_sel  CVWL668T.lib(drv_pwr.o)
    0x000172c8   0x000172c8   0x00000028   Code   RO         1040    i.drv_pwr_set_digit_power_sel  CVWL668T.lib(drv_pwr.o)
    0x000172f0   0x000172f0   0x00000034   Code   RO         1043    i.drv_pwr_set_pll_clk  CVWL668T.lib(drv_pwr.o)
    0x00017324   0x00017324   0x0000002c   Code   RO         1047    i.drv_pwr_set_wakeup_type  CVWL668T.lib(drv_pwr.o)
    0x00017350   0x00017350   0x00000020   Code   RO         1050    i.drv_pwr_write_lock  CVWL668T.lib(drv_pwr.o)
    0x00017370   0x00017370   0x00000010   Code   RO         1547    i.drv_rxbr_clear_pkt_buffer  CVWL668T.lib(drv_rxbr.o)
    0x00017380   0x00017380   0x0000000c   Code   RO         1548    i.drv_rxbr_clear_status0  CVWL668T.lib(drv_rxbr.o)
    0x0001738c   0x0001738c   0x0000005a   Code   RO         1551    i.drv_rxbr_enable_irq  CVWL668T.lib(drv_rxbr.o)
    0x000173e6   0x000173e6   0x00000002   PAD
    0x000173e8   0x000173e8   0x0000001c   Code   RO         1552    i.drv_rxbr_frame_drop_cfg  CVWL668T.lib(drv_rxbr.o)
    0x00017404   0x00017404   0x00000018   Code   RO          721    i.drv_rxbr_get_int_source  CVWL668T.lib(hal_internal_vsync.o)
    0x0001741c   0x0001741c   0x00000018   Code   RO          787    i.drv_rxbr_get_status0  CVWL668T.lib(hal_internal_dcs.o)
    0x00017434   0x00017434   0x00000014   Code   RO         1562    i.drv_rxbr_hline_rcv1_cfg  CVWL668T.lib(drv_rxbr.o)
    0x00017448   0x00017448   0x00000010   Code   RO         1563    i.drv_rxbr_hline_rcv_cfg  CVWL668T.lib(drv_rxbr.o)
    0x00017458   0x00017458   0x0000000c   Code   RO         1565    i.drv_rxbr_register_irq1_callback  CVWL668T.lib(drv_rxbr.o)
    0x00017464   0x00017464   0x00000018   Code   RO         1566    i.drv_rxbr_set_ack_pkt_header  CVWL668T.lib(drv_rxbr.o)
    0x0001747c   0x0001747c   0x0000001c   Code   RO         1571    i.drv_rxbr_set_color_format  CVWL668T.lib(drv_rxbr.o)
    0x00017498   0x00017498   0x00000024   Code   RO         1574    i.drv_rxbr_set_filter_regs  CVWL668T.lib(drv_rxbr.o)
    0x000174bc   0x000174bc   0x0000001c   Code   RO         1575    i.drv_rxbr_set_inten  CVWL668T.lib(drv_rxbr.o)
    0x000174d8   0x000174d8   0x00000018   Code   RO         1576    i.drv_rxbr_set_ltpo_drop_th  CVWL668T.lib(drv_rxbr.o)
    0x000174f0   0x000174f0   0x00000040   Code   RO         1580    i.drv_rxbr_set_usr_cfg  CVWL668T.lib(drv_rxbr.o)
    0x00017530   0x00017530   0x00000010   Code   RO         1581    i.drv_rxbr_set_usr_col  CVWL668T.lib(drv_rxbr.o)
    0x00017540   0x00017540   0x00000010   Code   RO         1582    i.drv_rxbr_set_usr_row  CVWL668T.lib(drv_rxbr.o)
    0x00017550   0x00017550   0x00000078   Code   RO         1204    i.drv_se_init       CVWL668T.lib(drv_se.o)
    0x000175c8   0x000175c8   0x000000d4   Code   RO         1205    i.drv_se_set_dsc    CVWL668T.lib(drv_se.o)
    0x0001769c   0x0001769c   0x00000088   Code   RO         1206    i.drv_se_set_lcdc   CVWL668T.lib(drv_se.o)
    0x00017724   0x00017724   0x00000068   Code   RO         1207    i.drv_se_set_memc   CVWL668T.lib(drv_se.o)
    0x0001778c   0x0001778c   0x000000d0   Code   RO         1208    i.drv_se_set_rxbr   CVWL668T.lib(drv_se.o)
    0x0001785c   0x0001785c   0x000000ac   Code   RO         1209    i.drv_se_set_vidc   CVWL668T.lib(drv_se.o)
    0x00017908   0x00017908   0x00000014   Code   RO         1210    i.drv_se_start_rx   CVWL668T.lib(drv_se.o)
    0x0001791c   0x0001791c   0x0000001c   Code   RO         1114    i.drv_swire_enable  CVWL668T.lib(drv_swire.o)
    0x00017938   0x00017938   0x0000000c   Code   RO         1115    i.drv_swire_get_pulse_count  CVWL668T.lib(drv_swire.o)
    0x00017944   0x00017944   0x0000000c   Code   RO         1116    i.drv_swire_register_callback  CVWL668T.lib(drv_swire.o)
    0x00017950   0x00017950   0x00000018   Code   RO         1117    i.drv_swire_set_bit_time  CVWL668T.lib(drv_swire.o)
    0x00017968   0x00017968   0x00000048   Code   RO         1118    i.drv_swire_set_int  CVWL668T.lib(drv_swire.o)
    0x000179b0   0x000179b0   0x0000001c   Code   RO         1119    i.drv_swire_set_power_down  CVWL668T.lib(drv_swire.o)
    0x000179cc   0x000179cc   0x0000000c   Code   RO         1120    i.drv_swire_set_pulse_count  CVWL668T.lib(drv_swire.o)
    0x000179d8   0x000179d8   0x0000001c   Code   RO         1121    i.drv_swire_set_trig_mode  CVWL668T.lib(drv_swire.o)
    0x000179f4   0x000179f4   0x0000000c   Code   RO         1136    i.drv_sys_cfg_clear_all_int  CVWL668T.lib(drv_sys_cfg.o)
    0x00017a00   0x00017a00   0x00000028   Code   RO         1137    i.drv_sys_cfg_clear_pending  CVWL668T.lib(drv_sys_cfg.o)
    0x00017a28   0x00017a28   0x00000024   Code   RO         1138    i.drv_sys_cfg_sel_ap_rst_trig  CVWL668T.lib(drv_sys_cfg.o)
    0x00017a4c   0x00017a4c   0x00000024   Code   RO         1140    i.drv_sys_cfg_sel_gpio_group  CVWL668T.lib(drv_sys_cfg.o)
    0x00017a70   0x00017a70   0x00000024   Code   RO         1141    i.drv_sys_cfg_sel_int_trig  CVWL668T.lib(drv_sys_cfg.o)
    0x00017a94   0x00017a94   0x00000018   Code   RO         1142    i.drv_sys_cfg_sel_swire_timer  CVWL668T.lib(drv_sys_cfg.o)
    0x00017aac   0x00017aac   0x00000024   Code   RO         1143    i.drv_sys_cfg_set_int  CVWL668T.lib(drv_sys_cfg.o)
    0x00017ad0   0x00017ad0   0x0000001a   Code   RO         1160    i.drv_timer_clear_status_flags  CVWL668T.lib(drv_timer.o)
    0x00017aea   0x00017aea   0x00000020   Code   RO         1161    i.drv_timer_enable  CVWL668T.lib(drv_timer.o)
    0x00017b0a   0x00017b0a   0x00000002   PAD
    0x00017b0c   0x00017b0c   0x00000010   Code   RO         1162    i.drv_timer_get_instance  CVWL668T.lib(drv_timer.o)
    0x00017b1c   0x00017b1c   0x0000003c   Code   RO         1164    i.drv_timer_handle_interrupt  CVWL668T.lib(drv_timer.o)
    0x00017b58   0x00017b58   0x00000040   Code   RO         1166    i.drv_timer_set_compare_val  CVWL668T.lib(drv_timer.o)
    0x00017b98   0x00017b98   0x00000048   Code   RO         1167    i.drv_timer_set_int  CVWL668T.lib(drv_timer.o)
    0x00017be0   0x00017be0   0x00000028   Code   RO         1168    i.drv_timer_set_prescaler  CVWL668T.lib(drv_timer.o)
    0x00017c08   0x00017c08   0x00000010   Code   RO         1169    i.drv_timer_set_repeat  CVWL668T.lib(drv_timer.o)
    0x00017c18   0x00017c18   0x00000020   Code   RO         1330    i.drv_tx_phy_test_enter  CVWL668T.lib(drv_dsi_tx.o)
    0x00017c38   0x00017c38   0x00000020   Code   RO         1331    i.drv_tx_phy_test_exit  CVWL668T.lib(drv_dsi_tx.o)
    0x00017c58   0x00017c58   0x00000028   Code   RO         1334    i.drv_tx_phy_test_write_code  CVWL668T.lib(drv_dsi_tx.o)
    0x00017c80   0x00017c80   0x00000034   Code   RO         1782    i.drv_uart_abort_recv  CVWL668T.lib(drv_uart.o)
    0x00017cb4   0x00017cb4   0x00000034   Code   RO         1783    i.drv_uart_abort_send  CVWL668T.lib(drv_uart.o)
    0x00017ce8   0x00017ce8   0x00000014   Code   RO         1784    i.drv_uart_config_int  CVWL668T.lib(drv_uart.o)
    0x00017cfc   0x00017cfc   0x00000018   Code   RO         1786    i.drv_uart_enable_clk  CVWL668T.lib(drv_uart.o)
    0x00017d14   0x00017d14   0x0000005c   Code   RO         1787    i.drv_uart_enable_int  CVWL668T.lib(drv_uart.o)
    0x00017d70   0x00017d70   0x00000028   Code   RO         1789    i.drv_uart_get_instance  CVWL668T.lib(drv_uart.o)
    0x00017d98   0x00017d98   0x000000ce   Code   RO         1790    i.drv_uart_init     CVWL668T.lib(drv_uart.o)
    0x00017e66   0x00017e66   0x00000002   PAD
    0x00017e68   0x00017e68   0x0000003c   Code   RO         1791    i.drv_uart_int_trans_handle  CVWL668T.lib(drv_uart.o)
    0x00017ea4   0x00017ea4   0x0000001c   Code   RO         1794    i.drv_uart_reset_rx_fifo  CVWL668T.lib(drv_uart.o)
    0x00017ec0   0x00017ec0   0x0000001c   Code   RO         1795    i.drv_uart_reset_tx_fifo  CVWL668T.lib(drv_uart.o)
    0x00017edc   0x00017edc   0x0000001a   Code   RO         1796    i.drv_uart_send_blocking  CVWL668T.lib(drv_uart.o)
    0x00017ef6   0x00017ef6   0x00000054   Code   RO         1798    i.drv_uart_set_baud_rate  CVWL668T.lib(drv_uart.o)
    0x00017f4a   0x00017f4a   0x00000002   PAD
    0x00017f4c   0x00017f4c   0x0000004c   Code   RO         1799    i.drv_uart_trans_create_handle  CVWL668T.lib(drv_uart.o)
    0x00017f98   0x00017f98   0x00000010   Code   RO         1634    i.drv_vidc_clear_irq  CVWL668T.lib(drv_vidc.o)
    0x00017fa8   0x00017fa8   0x00000020   Code   RO         1638    i.drv_vidc_enable   CVWL668T.lib(drv_vidc.o)
    0x00017fc8   0x00017fc8   0x00000040   Code   RO         1639    i.drv_vidc_enable_irq  CVWL668T.lib(drv_vidc.o)
    0x00018008   0x00018008   0x0000002c   Code   RO         1640    i.drv_vidc_get_int_source  CVWL668T.lib(drv_vidc.o)
    0x00018034   0x00018034   0x00000018   Code   RO         1641    i.drv_vidc_get_irq_status  CVWL668T.lib(drv_vidc.o)
    0x0001804c   0x0001804c   0x0000002c   Code   RO         1645    i.drv_vidc_init_module_enable  CVWL668T.lib(drv_vidc.o)
    0x00018078   0x00018078   0x0000000c   Code   RO         1646    i.drv_vidc_register_callback  CVWL668T.lib(drv_vidc.o)
    0x00018084   0x00018084   0x0000000c   Code   RO         1647    i.drv_vidc_reset    CVWL668T.lib(drv_vidc.o)
    0x00018090   0x00018090   0x0000001c   Code   RO         1648    i.drv_vidc_set_circ_mode_enable  CVWL668T.lib(drv_vidc.o)
    0x000180ac   0x000180ac   0x00000038   Code   RO         1649    i.drv_vidc_set_dither_config  CVWL668T.lib(drv_vidc.o)
    0x000180e4   0x000180e4   0x0000005c   Code   RO         1651    i.drv_vidc_set_dst_parameter  CVWL668T.lib(drv_vidc.o)
    0x00018140   0x00018140   0x0000000c   Code   RO         1653    i.drv_vidc_set_honly_hcoef0  CVWL668T.lib(drv_vidc.o)
    0x0001814c   0x0001814c   0x0000002c   Code   RO         1654    i.drv_vidc_set_honly_hinitb  CVWL668T.lib(drv_vidc.o)
    0x00018178   0x00018178   0x00000030   Code   RO         1655    i.drv_vidc_set_honly_hinitr  CVWL668T.lib(drv_vidc.o)
    0x000181a8   0x000181a8   0x0000001c   Code   RO         1658    i.drv_vidc_set_irqen  CVWL668T.lib(drv_vidc.o)
    0x000181c4   0x000181c4   0x00000014   Code   RO         1659    i.drv_vidc_set_mirror  CVWL668T.lib(drv_vidc.o)
    0x000181d8   0x000181d8   0x0000001c   Code   RO         1662    i.drv_vidc_set_pentile_swap  CVWL668T.lib(drv_vidc.o)
    0x000181f4   0x000181f4   0x0000000c   Code   RO         1663    i.drv_vidc_set_pu_ctrl  CVWL668T.lib(drv_vidc.o)
    0x00018200   0x00018200   0x00000018   Code   RO         1664    i.drv_vidc_set_rotation  CVWL668T.lib(drv_vidc.o)
    0x00018218   0x00018218   0x0000000c   Code   RO         1665    i.drv_vidc_set_scld_hcoef0  CVWL668T.lib(drv_vidc.o)
    0x00018224   0x00018224   0x0000000c   Code   RO         1666    i.drv_vidc_set_scld_hcoef1  CVWL668T.lib(drv_vidc.o)
    0x00018230   0x00018230   0x00000014   Code   RO         1667    i.drv_vidc_set_scld_step  CVWL668T.lib(drv_vidc.o)
    0x00018244   0x00018244   0x0000000c   Code   RO         1668    i.drv_vidc_set_scld_vcoef0  CVWL668T.lib(drv_vidc.o)
    0x00018250   0x00018250   0x0000000c   Code   RO         1669    i.drv_vidc_set_scld_vcoef1  CVWL668T.lib(drv_vidc.o)
    0x0001825c   0x0001825c   0x00000020   Code   RO         1670    i.drv_vidc_set_src_parameter  CVWL668T.lib(drv_vidc.o)
    0x0001827c   0x0001827c   0x00000038   Code   RO         1671    i.drv_vidc_set_vintp_config  CVWL668T.lib(drv_vidc.o)
    0x000182b4   0x000182b4   0x00000034   Code   RO          671    i.fputc             CVWL668T.lib(tau_log.o)
    0x000182e8   0x000182e8   0x00000060   Code   RO          115    i.google_p6a_demo   p6a_demo.o
    0x00018348   0x00018348   0x00000040   Code   RO          815    i.ha_intl_fb_check_pu_size  CVWL668T.lib(hal_internal_fb.o)
    0x00018388   0x00018388   0x00000040   Code   RO          321    i.hal_dsi_rx_ctrl_create_handle  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x000183c8   0x000183c8   0x00000040   Code   RO          322    i.hal_dsi_rx_ctrl_dcs_async_handler  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00018408   0x00018408   0x00000094   Code   RO          323    i.hal_dsi_rx_ctrl_deinit  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x0001849c   0x0001849c   0x00000020   Code   RO          330    i.hal_dsi_rx_ctrl_get_max_ret_size  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x000184bc   0x000184bc   0x000000ac   Code   RO          331    i.hal_dsi_rx_ctrl_init  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00018568   0x00018568   0x00000100   Code   RO          332    i.hal_dsi_rx_ctrl_init_clk  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00018668   0x00018668   0x00000108   Code   RO          333    i.hal_dsi_rx_ctrl_init_dsi_rx  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00018770   0x00018770   0x0000012c   Code   RO          334    i.hal_dsi_rx_ctrl_init_memc  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x0001889c   0x0001889c   0x00000148   Code   RO          335    i.hal_dsi_rx_ctrl_init_rxbr  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x000189e4   0x000189e4   0x00000280   Code   RO          336    i.hal_dsi_rx_ctrl_init_vidc  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00018c64   0x00018c64   0x00000038   Code   RO          337    i.hal_dsi_rx_ctrl_pre_init_pps  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00018c9c   0x00018c9c   0x000000f0   Code   RO          342    i.hal_dsi_rx_ctrl_send_ack_cmd  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00018d8c   0x00018d8c   0x00000030   Code   RO          349    i.hal_dsi_rx_ctrl_set_ipi_cfg  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00018dbc   0x00018dbc   0x00000030   Code   RO          355    i.hal_dsi_rx_ctrl_start  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00018dec   0x00018dec   0x00000030   Code   RO          356    i.hal_dsi_rx_ctrl_stop  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00018e1c   0x00018e1c   0x00000020   Code   RO          358    i.hal_dsi_rx_ctrl_toggle_resolution  CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00018e3c   0x00018e3c   0x00000280   Code   RO          411    i.hal_dsi_tx_cmd_mode_cal_timing  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x000190bc   0x000190bc   0x00000038   Code   RO          413    i.hal_dsi_tx_ctrl_create_handle  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x000190f4   0x000190f4   0x00000074   Code   RO          414    i.hal_dsi_tx_ctrl_deinit  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00019168   0x00019168   0x00000022   Code   RO          417    i.hal_dsi_tx_ctrl_gen_a_tear_signal  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001918a   0x0001918a   0x00000002   PAD
    0x0001918c   0x0001918c   0x0000007c   Code   RO          419    i.hal_dsi_tx_ctrl_init  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00019208   0x00019208   0x00000010   Code   RO          420    i.hal_dsi_tx_ctrl_init_clk  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00019218   0x00019218   0x00000008   Code   RO          433    i.hal_dsi_tx_ctrl_set_overwrite_rgb  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00019220   0x00019220   0x0000000a   Code   RO          434    i.hal_dsi_tx_ctrl_set_tear_mode  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001922a   0x0001922a   0x00000002   PAD
    0x0001922c   0x0001922c   0x00000090   Code   RO          436    i.hal_dsi_tx_ctrl_start  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x000192bc   0x000192bc   0x00000038   Code   RO          437    i.hal_dsi_tx_ctrl_stop  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x000192f4   0x000192f4   0x000000d0   Code   RO          440    i.hal_dsi_tx_ctrl_write_cmd  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x000193c4   0x000193c4   0x00000104   Code   RO          441    i.hal_dsi_tx_init_cfg  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x000194c8   0x000194c8   0x00000044   Code   RO          442    i.hal_dsi_tx_init_dpi_timing  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001950c   0x0001950c   0x00000016   Code   RO          443    i.hal_dsi_tx_init_phy_cfg  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00019522   0x00019522   0x00000052   Code   RO          444    i.hal_dsi_tx_init_timing  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00019574   0x00019574   0x00000054   Code   RO          445    i.hal_dsi_tx_init_vid_timing  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x000195c8   0x000195c8   0x00000040   Code   RO          446    i.hal_dsi_tx_send_cmd  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00019608   0x00019608   0x00000094   Code   RO          447    i.hal_dsi_tx_timing_info_update  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001969c   0x0001969c   0x00000310   Code   RO          448    i.hal_dsi_tx_vid_mode_cal_timing  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x000199ac   0x000199ac   0x0000003a   Code   RO          518    i.hal_gpio_config_pad  CVWL668T.lib(hal_gpio.o)
    0x000199e6   0x000199e6   0x00000002   PAD
    0x000199e8   0x000199e8   0x00000018   Code   RO          519    i.hal_gpio_ctrl_eint  CVWL668T.lib(hal_gpio.o)
    0x00019a00   0x00019a00   0x00000040   Code   RO          523    i.hal_gpio_init_eint  CVWL668T.lib(hal_gpio.o)
    0x00019a40   0x00019a40   0x00000016   Code   RO          524    i.hal_gpio_init_input  CVWL668T.lib(hal_gpio.o)
    0x00019a56   0x00019a56   0x0000001c   Code   RO          525    i.hal_gpio_init_output  CVWL668T.lib(hal_gpio.o)
    0x00019a72   0x00019a72   0x00000002   PAD
    0x00019a74   0x00019a74   0x0000001c   Code   RO          526    i.hal_gpio_reg_eint_cb  CVWL668T.lib(hal_gpio.o)
    0x00019a90   0x00019a90   0x00000050   Code   RO          527    i.hal_gpio_set_ap_reset_int  CVWL668T.lib(hal_gpio.o)
    0x00019ae0   0x00019ae0   0x00000060   Code   RO          530    i.hal_gpio_set_mode  CVWL668T.lib(hal_gpio.o)
    0x00019b40   0x00019b40   0x00000008   Code   RO          531    i.hal_gpio_set_output_data  CVWL668T.lib(hal_gpio.o)
    0x00019b48   0x00019b48   0x00000010   Code   RO          723    i.hal_internal_sync_get_hight_performan_mode  CVWL668T.lib(hal_internal_vsync.o)
    0x00019b58   0x00019b58   0x000001b4   Code   RO          724    i.hal_internal_sync_input_resolution_change  CVWL668T.lib(hal_internal_vsync.o)
    0x00019d0c   0x00019d0c   0x0000000c   Code   RO          725    i.hal_internal_sync_register_lcdc_cb  CVWL668T.lib(hal_internal_vsync.o)
    0x00019d18   0x00019d18   0x00000020   Code   RO          728    i.hal_internal_vsync_deinit  CVWL668T.lib(hal_internal_vsync.o)
    0x00019d38   0x00019d38   0x0000000c   Code   RO          729    i.hal_internal_vsync_get_rx_state  CVWL668T.lib(hal_internal_vsync.o)
    0x00019d44   0x00019d44   0x00000014   Code   RO          730    i.hal_internal_vsync_get_sync_line  CVWL668T.lib(hal_internal_vsync.o)
    0x00019d58   0x00019d58   0x0000000c   Code   RO          731    i.hal_internal_vsync_get_tx_state  CVWL668T.lib(hal_internal_vsync.o)
    0x00019d64   0x00019d64   0x000000e8   Code   RO          732    i.hal_internal_vsync_init_rx  CVWL668T.lib(hal_internal_vsync.o)
    0x00019e4c   0x00019e4c   0x000000c8   Code   RO          733    i.hal_internal_vsync_init_tx  CVWL668T.lib(hal_internal_vsync.o)
    0x00019f14   0x00019f14   0x00000020   Code   RO          734    i.hal_internal_vsync_set_rx_state  CVWL668T.lib(hal_internal_vsync.o)
    0x00019f34   0x00019f34   0x000001ec   Code   RO          736    i.hal_internal_vsync_set_tear_mode  CVWL668T.lib(hal_internal_vsync.o)
    0x0001a120   0x0001a120   0x00000058   Code   RO          737    i.hal_internal_vsync_set_tx_state  CVWL668T.lib(hal_internal_vsync.o)
    0x0001a178   0x0001a178   0x0000006c   Code   RO          788    i.hal_intl_dcs_init_sw_fltr  CVWL668T.lib(hal_internal_dcs.o)
    0x0001a1e4   0x0001a1e4   0x00000430   Code   RO          790    i.hal_intl_dcs_rx_get_dcs_packet_data  CVWL668T.lib(hal_internal_dcs.o)
    0x0001a614   0x0001a614   0x00000088   Code   RO          791    i.hal_intl_dcs_rx_receive_packet  CVWL668T.lib(hal_internal_dcs.o)
    0x0001a69c   0x0001a69c   0x00000174   Code   RO          792    i.hal_intl_dcs_rx_receive_pps  CVWL668T.lib(hal_internal_dcs.o)
    0x0001a810   0x0001a810   0x0000008c   Code   RO          793    i.hal_intl_dcs_set_auto_hw_filter  CVWL668T.lib(hal_internal_dcs.o)
    0x0001a89c   0x0001a89c   0x0000002c   Code   RO          795    i.hal_intl_dcs_sw_filter_handle  CVWL668T.lib(hal_internal_dcs.o)
    0x0001a8c8   0x0001a8c8   0x00000318   Code   RO          816    i.hal_intl_fb_cal_fb_info  CVWL668T.lib(hal_internal_fb.o)
    0x0001abe0   0x0001abe0   0x00000064   Code   RO          817    i.hal_intl_fb_check_bandwidth  CVWL668T.lib(hal_internal_fb.o)
    0x0001ac44   0x0001ac44   0x000000dc   Code   RO          818    i.hal_intl_fb_edge_resize  CVWL668T.lib(hal_internal_fb.o)
    0x0001ad20   0x0001ad20   0x00000074   Code   RO          819    i.hal_intl_fb_flow_control_adapter  CVWL668T.lib(hal_internal_fb.o)
    0x0001ad94   0x0001ad94   0x0000000c   Code   RO          820    i.hal_intl_fb_get_memc_flow_mode  CVWL668T.lib(hal_internal_fb.o)
    0x0001ada0   0x0001ada0   0x00000010   Code   RO          821    i.hal_intl_fb_get_rx_fb_info  CVWL668T.lib(hal_internal_fb.o)
    0x0001adb0   0x0001adb0   0x00000010   Code   RO          822    i.hal_intl_fb_get_tx_fb_info  CVWL668T.lib(hal_internal_fb.o)
    0x0001adc0   0x0001adc0   0x0000000c   Code   RO          823    i.hal_intl_fb_get_user_flow  CVWL668T.lib(hal_internal_fb.o)
    0x0001adcc   0x0001adcc   0x00000028   Code   RO          841    i.hal_intl_svs_deinit_rx  CVWL668T.lib(hal_internal_svs.o)
    0x0001adf4   0x0001adf4   0x00000010   Code   RO          842    i.hal_intl_svs_deinit_tx  CVWL668T.lib(hal_internal_svs.o)
    0x0001ae04   0x0001ae04   0x00000024   Code   RO          843    i.hal_intl_svs_handle  CVWL668T.lib(hal_internal_svs.o)
    0x0001ae28   0x0001ae28   0x00000080   Code   RO          844    i.hal_intl_svs_init_rx  CVWL668T.lib(hal_internal_svs.o)
    0x0001aea8   0x0001aea8   0x00000014   Code   RO          845    i.hal_intl_svs_init_tx  CVWL668T.lib(hal_internal_svs.o)
    0x0001aebc   0x0001aebc   0x0000000c   Code   RO          847    i.hal_intl_svs_set_rx_vtt  CVWL668T.lib(hal_internal_svs.o)
    0x0001aec8   0x0001aec8   0x00000048   Code   RO          849    i.hal_intl_svs_update_rxbr_clk  CVWL668T.lib(hal_internal_svs.o)
    0x0001af10   0x0001af10   0x00000070   Code   RO          449    i.hal_lcdc_displayproc_config  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001af80   0x0001af80   0x0000003e   Code   RO          450    i.hal_lcdc_init_cfg  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001afbe   0x0001afbe   0x00000070   Code   RO          451    i.hal_lcdc_init_clk  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001b02e   0x0001b02e   0x00000002   PAD
    0x0001b030   0x0001b030   0x00000128   Code   RO          452    i.hal_lcdc_postproc_config  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001b158   0x0001b158   0x00000024   Code   RO          453    i.hal_lcdc_start    CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001b17c   0x0001b17c   0x0000003c   Code   RO          454    i.hal_lcdc_timinggen_config  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001b1b8   0x0001b1b8   0x000000e0   Code   RO          455    i.hal_lcdc_upscaler_config  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001b298   0x0001b298   0x000000bc   Code   RO          457    i.hal_nonshadow_func_update  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001b354   0x0001b354   0x0000002a   Code   RO          622    i.hal_pwr_enter_deep_sleep_mode  CVWL668T.lib(hal_pwr.o)
    0x0001b37e   0x0001b37e   0x00000008   Code   RO          623    i.hal_pwr_enter_normal_sleep_mode  CVWL668T.lib(hal_pwr.o)
    0x0001b386   0x0001b386   0x00000002   PAD
    0x0001b388   0x0001b388   0x00000064   Code   RO          624    i.hal_pwr_enter_stop_sleep_mode  CVWL668T.lib(hal_pwr.o)
    0x0001b3ec   0x0001b3ec   0x0000000a   Code   RO          625    i.hal_pwr_exit_sleep_mode  CVWL668T.lib(hal_pwr.o)
    0x0001b3f6   0x0001b3f6   0x00000008   Code   RO          627    i.hal_pwr_get_vcc_power_ready  CVWL668T.lib(hal_pwr.o)
    0x0001b3fe   0x0001b3fe   0x00000008   Code   RO          632    i.hal_pwr_set_main_power  CVWL668T.lib(hal_pwr.o)
    0x0001b406   0x0001b406   0x00000008   Code   RO          634    i.hal_pwr_set_sleep_mode_power  CVWL668T.lib(hal_pwr.o)
    0x0001b40e   0x0001b40e   0x00000002   PAD
    0x0001b410   0x0001b410   0x00000064   Code   RO          635    i.hal_pwr_set_stop_sleep_wakeup_pin  CVWL668T.lib(hal_pwr.o)
    0x0001b474   0x0001b474   0x00000040   Code   RO          558    i.hal_swire_deinit  CVWL668T.lib(hal_swire.o)
    0x0001b4b4   0x0001b4b4   0x0000005c   Code   RO          559    i.hal_swire_enable  CVWL668T.lib(hal_swire.o)
    0x0001b510   0x0001b510   0x00000058   Code   RO          560    i.hal_swire_init    CVWL668T.lib(hal_swire.o)
    0x0001b568   0x0001b568   0x00000024   Code   RO          562    i.hal_swire_set_pulse  CVWL668T.lib(hal_swire.o)
    0x0001b58c   0x0001b58c   0x00000040   Code   RO          563    i.hal_swire_set_timer  CVWL668T.lib(hal_swire.o)
    0x0001b5cc   0x0001b5cc   0x000000e4   Code   RO          583    i.hal_system_init   CVWL668T.lib(hal_system.o)
    0x0001b6b0   0x0001b6b0   0x00000050   Code   RO          586    i.hal_system_updata_sysclk  CVWL668T.lib(hal_system.o)
    0x0001b700   0x0001b700   0x00000030   Code   RO          601    i.hal_timer_deinit  CVWL668T.lib(hal_timer.o)
    0x0001b730   0x0001b730   0x0000001c   Code   RO          603    i.hal_timer_init    CVWL668T.lib(hal_timer.o)
    0x0001b74c   0x0001b74c   0x00000008   Code   RO          604    i.hal_timer_set_repeat  CVWL668T.lib(hal_timer.o)
    0x0001b754   0x0001b754   0x00000030   Code   RO          458    i.hal_tx_frame_rate_adjust  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001b784   0x0001b784   0x00000094   Code   RO          695    i.hal_uart_init     CVWL668T.lib(hal_uart.o)
    0x0001b818   0x0001b818   0x0000001c   Code   RO          698    i.hal_uart_send_blocking  CVWL668T.lib(hal_uart.o)
    0x0001b834   0x0001b834   0x00000018   Code   RO          459    i.hal_vsync_func_update  CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001b84c   0x0001b84c   0x000000e0   Code   RO          739    i.hal_vsync_reset_lcdc_scaler  CVWL668T.lib(hal_internal_vsync.o)
    0x0001b92c   0x0001b92c   0x00000040   Code   RO            3    i.main              main.o
    0x0001b96c   0x0001b96c   0x0000007c   Code   RO          116    i.pps_update_handle  p6a_demo.o
    0x0001b9e8   0x0001b9e8   0x000002e4   Code   RO          740    i.rxbr_irq1_callback  CVWL668T.lib(hal_internal_vsync.o)
    0x0001bccc   0x0001bccc   0x00000044   Code   RO          741    i.soft_double_buffer_update  CVWL668T.lib(hal_internal_vsync.o)
    0x0001bd10   0x0001bd10   0x0000006c   Code   RO          742    i.soft_gen_te       CVWL668T.lib(hal_internal_vsync.o)
    0x0001bd7c   0x0001bd7c   0x000000e0   Code   RO          743    i.soft_gen_te_double_buffer  CVWL668T.lib(hal_internal_vsync.o)
    0x0001be5c   0x0001be5c   0x00000038   Code   RO          744    i.soft_pro_motion_init  CVWL668T.lib(hal_internal_vsync.o)
    0x0001be94   0x0001be94   0x00000024   Code   RO          745    i.soft_tear_adjust_line  CVWL668T.lib(hal_internal_vsync.o)
    0x0001beb8   0x0001beb8   0x00000018   Code   RO          637    i.stop_sleep_cb     CVWL668T.lib(hal_pwr.o)
    0x0001bed0   0x0001bed0   0x000000ac   Code   RO          850    i.svs_direct_mode_setting  CVWL668T.lib(hal_internal_svs.o)
    0x0001bf7c   0x0001bf7c   0x0000001c   Code   RO          851    i.svs_get_rel_intv  CVWL668T.lib(hal_internal_svs.o)
    0x0001bf98   0x0001bf98   0x000000b0   Code   RO          852    i.svs_sync_handle   CVWL668T.lib(hal_internal_svs.o)
    0x0001c048   0x0001c048   0x000000cc   Code   RO          853    i.svs_wait_fr_stab  CVWL668T.lib(hal_internal_svs.o)
    0x0001c114   0x0001c114   0x0000010c   Code   RO          854    i.svs_wait_start    CVWL668T.lib(hal_internal_svs.o)
    0x0001c220   0x0001c220   0x00000034   Code   RO          672    i.tau_log_init      CVWL668T.lib(tau_log.o)
    0x0001c254   0x0001c254   0x00000084   Code   RO          673    i.tau_log_printf    CVWL668T.lib(tau_log.o)
    0x0001c2d8   0x0001c2d8   0x00000076   Code   RO          674    i.tau_log_push_log  CVWL668T.lib(tau_log.o)
    0x0001c34e   0x0001c34e   0x00000002   PAD
    0x0001c350   0x0001c350   0x000000b4   Code   RO          746    i.vidc_callback     CVWL668T.lib(hal_internal_vsync.o)
    0x0001c404   0x0001c404   0x00000118   Code   RO          747    i.vpre_err_reset    CVWL668T.lib(hal_internal_vsync.o)
    0x0001c51c   0x0001c51c   0x00000058   Data   RO          119    .constdata          p6a_demo.o
    0x0001c574   0x0001c574   0x00000028   Data   RO          361    .constdata          CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x0001c59c   0x0001c59c   0x0000001c   Data   RO          462    .constdata          CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0001c5b8   0x0001c5b8   0x000000b6   Data   RO          535    .constdata          CVWL668T.lib(hal_gpio.o)
    0x0001c66e   0x0001c66e   0x00000002   PAD
    0x0001c670   0x0001c670   0x00000030   Data   RO          700    .constdata          CVWL668T.lib(hal_uart.o)
    0x0001c6a0   0x0001c6a0   0x00000010   Data   RO         1801    .constdata          CVWL668T.lib(drv_uart.o)
    0x0001c6b0   0x0001c6b0   0x00000042   Data   RO          362    .conststring        CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x0001c6f2   0x0001c6f2   0x00000002   PAD
    0x0001c6f4   0x0001c6f4   0x00000090   Data   RO          749    .conststring        CVWL668T.lib(hal_internal_vsync.o)
    0x0001c784   0x0001c784   0x00000046   Data   RO          798    .conststring        CVWL668T.lib(hal_internal_dcs.o)
    0x0001c7ca   0x0001c7ca   0x00000002   PAD
    0x0001c7cc   0x0001c7cc   0x00000020   Data   RO         2215    Region$$Table       anon$$obj.o


    Execution Region RW_IRAM1 (Exec base: 0x00070000, Load base: 0x0001c7ec, Size: 0x00003108, Max: 0x00008000, ABSOLUTE, COMPRESSED[0x0000014c])

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00070000   COMPRESSED   0x0000009f   Data   RW          120    .data               p6a_demo.o
    0x0007009f   COMPRESSED   0x00000001   PAD
    0x000700a0   COMPRESSED   0x00000030   Data   RW          363    .data               CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x000700d0   COMPRESSED   0x0000005c   Data   RW          463    .data               CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x0007012c   COMPRESSED   0x00000002   Data   RW          565    .data               CVWL668T.lib(hal_swire.o)
    0x0007012e   COMPRESSED   0x00000002   PAD
    0x00070130   COMPRESSED   0x00000008   Data   RW          638    .data               CVWL668T.lib(hal_pwr.o)
    0x00070138   COMPRESSED   0x00000001   Data   RW          677    .data               CVWL668T.lib(tau_log.o)
    0x00070139   COMPRESSED   0x00000003   PAD
    0x0007013c   COMPRESSED   0x00000018   Data   RW          701    .data               CVWL668T.lib(hal_uart.o)
    0x00070154   COMPRESSED   0x00000010   Data   RW          750    .data               CVWL668T.lib(hal_internal_vsync.o)
    0x00070164   COMPRESSED   0x00000024   Data   RW          799    .data               CVWL668T.lib(hal_internal_dcs.o)
    0x00070188   COMPRESSED   0x0000000c   Data   RW          883    .data               CVWL668T.lib(drv_common.o)
    0x00070194   COMPRESSED   0x00000001   Data   RW          884    .data               CVWL668T.lib(drv_common.o)
    0x00070195   COMPRESSED   0x00000003   PAD
    0x00070198   COMPRESSED   0x00000004   Data   RW          970    .data               CVWL668T.lib(drv_gpio.o)
    0x0007019c   COMPRESSED   0x00000004   Data   RW         1122    .data               CVWL668T.lib(drv_swire.o)
    0x000701a0   COMPRESSED   0x00000050   Data   RW         1170    .data               CVWL668T.lib(drv_timer.o)
    0x000701f0   COMPRESSED   0x00000004   Data   RW         1211    .data               CVWL668T.lib(drv_se.o)
    0x000701f4   COMPRESSED   0x00000001   Data   RW         1251    .data               CVWL668T.lib(drv_dsi_rx.o)
    0x000701f5   COMPRESSED   0x00000003   PAD
    0x000701f8   COMPRESSED   0x00000008   Data   RW         1586    .data               CVWL668T.lib(drv_rxbr.o)
    0x00070200   COMPRESSED   0x00000004   Data   RW         1673    .data               CVWL668T.lib(drv_vidc.o)
    0x00070204   COMPRESSED   0x00000190   Data   RW         1748    .data               CVWL668T.lib(drv_dma.o)
    0x00070394   COMPRESSED   0x00000004   Data   RW         2191    .data               mc_p.l(stdout.o)
    0x00070398        -       0x000000d0   Zero   RW          360    .bss                CVWL668T.lib(hal_dsi_rx_ctrl.o)
    0x00070468        -       0x000000b8   Zero   RW          461    .bss                CVWL668T.lib(hal_dsi_tx_ctrl.o)
    0x00070520        -       0x00000100   Zero   RW          676    .bss                CVWL668T.lib(tau_log.o)
    0x00070620        -       0x00000044   Zero   RW          748    .bss                CVWL668T.lib(hal_internal_vsync.o)
    0x00070664        -       0x00000800   Zero   RW          796    .bss                CVWL668T.lib(hal_internal_dcs.o)
    0x00070e64        -       0x000000ff   Zero   RW          797    .bss                CVWL668T.lib(hal_internal_dcs.o)
    0x00070f63   COMPRESSED   0x00000001   PAD
    0x00070f64        -       0x00000044   Zero   RW          825    .bss                CVWL668T.lib(hal_internal_fb.o)
    0x00070fa8        -       0x00000044   Zero   RW          855    .bss                CVWL668T.lib(hal_internal_svs.o)
    0x00070fec        -       0x00000040   Zero   RW          969    .bss                CVWL668T.lib(drv_gpio.o)
    0x0007102c        -       0x0000106c   Zero   RW         1194    .bss                CVWL668T.lib(dcs_packet_fifo.o)
    0x00072098        -       0x00000010   Zero   RW         1746    .bss                CVWL668T.lib(drv_dma.o)
    0x000720a8        -       0x00000060   Zero   RW         1800    .bss                CVWL668T.lib(drv_uart.o)
    0x00072108        -       0x00001000   Zero   RW          310    STACK               startup_armcm0.o


==============================================================================

Image component sizes


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Object Name

        24          4          0          0          0        581   board.o
        64         32          0          0          0      10487   main.o
     15582        802         88        159          0      29960   p6a_demo.o
       120         18        192          0       4096       2168   startup_armcm0.o

    ----------------------------------------------------------------------
     15792        856        312        160       4096      43196   Object Totals
         0          0         32          0          0          0   (incl. Generated)
         2          0          0          1          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Member Name

       216         32          0          0       4204        252   dcs_packet_fifo.o
       104         62         28         13          0        192   drv_common.o
       536         90          0          0          0        792   drv_crgu.o
       136         22          0        400         16        196   drv_dma.o
       144         34          0          0          0        248   drv_dsc_dec.o
      1904        682          0          1          0       1340   drv_dsi_rx.o
      1704        306          0          0          0       2036   drv_dsi_tx.o
       148          0          0          0          0        260   drv_efuse.o
       296         40          0          4         64       1000   drv_gpio.o
      1080        166          0          0          0       1620   drv_lcdc.o
       658        104          0          0          0       1240   drv_memc.o
        40          0          0          0          0        120   drv_phy_common.o
       592        132          0          0          0        716   drv_pwr.o
       514        102          0          8          0       1120   drv_rxbr.o
       972        266          0          4          0        488   drv_se.o
       264         54          0          4          0        560   drv_swire.o
       220         40          0          0          0        428   drv_sys_cfg.o
       366         38          0         80          0        816   drv_timer.o
      1172         54         16          0         96        980   drv_uart.o
       824        152          0          4          0       1700   drv_vidc.o
      2766        204        106         48        208       1256   hal_dsi_rx_ctrl.o
      4086        332         50         92        184       2128   hal_dsi_tx_ctrl.o
       440         32        182          0          0        688   hal_gpio.o
      2140        506         70         36       2303        652   hal_internal_dcs.o
      1348         58          0          0         68        700   hal_internal_fb.o
      1172        182          0          0         68        840   hal_internal_svs.o
      3824        804        144         16         68       1688   hal_internal_vsync.o
       308         32          0          8          0        616   hal_pwr.o
       344         32          0          2          0        348   hal_swire.o
       308         56          0          0          0        136   hal_system.o
        84          0          0          0          0        204   hal_timer.o
       176         18         48         24          0        144   hal_uart.o
        68          4          0          0          0        136   tau_delay.o
       354         30         16          1        256        320   tau_log.o
       200         20          0          0          0         76   ceil.o
        86          0          0          0          0          0   __dczerorl2.o
         0          0          0          0          0          0   entry.o
         0          0          0          0          0          0   entry10a.o
         0          0          0          0          0          0   entry11a.o
         8          4          0          0          0          0   entry2.o
         4          0          0          0          0          0   entry5.o
         0          0          0          0          0          0   entry7b.o
         0          0          0          0          0          0   entry8b.o
         8          4          0          0          0          0   entry9a.o
        30          0          0          0          0          0   handlers.o
        40          0          0          0          0         72   idiv.o
        36          8          0          0          0         68   init.o
         0          0          0          0          0          0   iusefp.o
        32          0          0          0          0         68   llshl.o
        38          0          0          0          0         68   llsshr.o
        34          0          0          0          0         68   llushr.o
        26          0          0          0          0         72   memcmp.o
        36          0          0          0          0         60   memcpya.o
        36          0          0          0          0        100   memseta.o
      2298        104          0          0          0        544   printfa.o
         0          0          0          4          0          0   stdout.o
        14          0          0          0          0         60   strlen.o
        44          0          0          0          0         72   uidiv.o
        96          0          0          0          0         84   uldiv.o
        40          2          0          0          0         68   cdrcmple.o
        20          0          0          0          0         68   cfcmple.o
        20          0          0          0          0         68   cfrcmple.o
        56          0          0          0          0         68   d2f.o
       356          4          0          0          0        140   dadd.o
       240          6          0          0          0         84   ddiv.o
       236          0          0          0          0        216   depilogue.o
        60         10          0          0          0         68   dfixui.o
        64         10          0          0          0         68   dfixul.o
        28          4          0          0          0         68   dfltui.o
       208          6          0          0          0         88   dmul.o
        40          0          0          0          0         60   f2d.o
       178          0          0          0          0        108   fadd.o
       124          0          0          0          0         72   fdiv.o
       130          0          0          0          0        144   fepilogue.o
        40          0          0          0          0         60   ffixui.o
        14          0          0          0          0         68   ffltui.o
       122          0          0          0          0         72   fmul.o
        24          0          0          0          0         60   fscalb.o

    ----------------------------------------------------------------------
     34408       4848        668        760       7536      29020   Library Totals
        34          0          8         11          1          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Name

     29308       4666        660        745       7535      25960   CVWL668T.lib
       200         20          0          0          0         76   m_ps.l
      2866        120          0          4          0       1336   mc_p.l
      2000         42          0          0          0       1648   mf_p.l

    ----------------------------------------------------------------------
     34408       4848        668        760       7536      29020   Library Totals

    ----------------------------------------------------------------------

==============================================================================


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   

     50200       5704        980        920      11632      52924   Grand Totals
     50200       5704        980        332      11632      52924   ELF Image Totals (compressed)
     50200       5704        980        332          0          0   ROM Totals

==============================================================================

    Total RO  Size (Code + RO Data)                51180 (  49.98kB)
    Total RW  Size (RW Data + ZI Data)             12552 (  12.26kB)
    Total ROM Size (Code + RO Data + RW Data)      51512 (  50.30kB)

==============================================================================

