Component: ARM Compiler 5.06 update 6 (build 750) Tool: armlink [4d35ed]

==============================================================================

Section Cross References

    main.o(i.main) refers to board.o(i.board_Init) for board_Init
    main.o(i.main) refers to ap_demo.o(i.ap_demo) for ap_demo
    ap_demo.o(i.Gpio_swire_output) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    ap_demo.o(i.Gpio_swire_output) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.Gpio_swire_output) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    ap_demo.o(i.Gpio_swire_output) refers to tau_delay.o(i.delayUs) for delayUs
    ap_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) for hal_dsi_rx_ctrl_send_ack_cmd
    ap_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) for hal_dsi_rx_ctrl_get_max_ret_size
    ap_demo.o(i.ap_dcs_read) refers to memcpya.o(.text) for __aeabi_memcpy4
    ap_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd) for hal_dsi_rx_ctrl_ack_long_cmd
    ap_demo.o(i.ap_dcs_read) refers to app_tp_st_touch.o(i.ap_get_tp_calibration_status_01) for ap_get_tp_calibration_status_01
    ap_demo.o(i.ap_dcs_read) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_dcs_read) refers to ap_demo.o(.data) for g_rx_ctrl_handle
    ap_demo.o(i.ap_dcs_read) refers to ap_demo.o(.constdata) for .constdata
    ap_demo.o(i.ap_demo) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.open_mipi_rx) for open_mipi_rx
    ap_demo.o(i.ap_demo) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.init_mipi_tx) for init_mipi_tx
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_init) for app_tp_init
    ap_demo.o(i.ap_demo) refers to hal_timer.o(i.hal_timer_init) for hal_timer_init
    ap_demo.o(i.ap_demo) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    ap_demo.o(i.ap_demo) refers to tau_delay.o(i.delayUs) for delayUs
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.tx_display_on) for tx_display_on
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_phone_clear_reset_on) for app_tp_phone_clear_reset_on
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_transfer_screen_start) for app_tp_transfer_screen_start
    ap_demo.o(i.ap_demo) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_transfer_screen_int) for app_tp_transfer_screen_int
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.tp_heartbeat_exec) for tp_heartbeat_exec
    ap_demo.o(i.ap_demo) refers to app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec) for ap_tp_st_touch_scan_point_record_event_exec
    ap_demo.o(i.ap_demo) refers to app_tp_st_touch.o(i.app_tp_calibration_exec) for app_tp_calibration_exec
    ap_demo.o(i.ap_demo) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) for hal_dsi_rx_ctrl_dsc_async_handler
    ap_demo.o(i.ap_demo) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) for hal_dsi_tx_ctrl_stop
    ap_demo.o(i.ap_demo) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) for hal_dsi_tx_ctrl_deinit
    ap_demo.o(i.ap_demo) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) for hal_dsi_rx_ctrl_stop
    ap_demo.o(i.ap_demo) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) for hal_dsi_rx_ctrl_deinit
    ap_demo.o(i.ap_demo) refers to hal_swire.o(i.hal_swire_open) for hal_swire_open
    ap_demo.o(i.ap_demo) refers to hal_swire.o(i.hal_swire_deinit) for hal_swire_deinit
    ap_demo.o(i.ap_demo) refers to hal_timer.o(i.hal_timer_stop) for hal_timer_stop
    ap_demo.o(i.ap_demo) refers to hal_timer.o(i.hal_timer_deinit) for hal_timer_deinit
    ap_demo.o(i.ap_demo) refers to hal_system.o(i.hal_system_set_vcc) for hal_system_set_vcc
    ap_demo.o(i.ap_demo) refers to ap_demo.o(.data) for phone_DisplayOFF_flag
    ap_demo.o(i.ap_demo) refers to app_tp_for_custom_s8.o(.data) for tp_sleep_count
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.soft_timer3_cb) for soft_timer3_cb
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.ap_reset_cb) for ap_reset_cb
    ap_demo.o(i.ap_get_51_reg) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_get_51_reg) refers to ap_demo.o(.data) for value_reg_51
    ap_demo.o(i.ap_get_67_reg) refers to uidiv.o(.text) for __aeabi_uidivmod
    ap_demo.o(i.ap_get_67_reg) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_get_67_reg) refers to ap_demo.o(.data) for value_reg_67
    ap_demo.o(i.ap_get_dcs) refers to ap_demo.o(i.set_soft_tear_mode) for set_soft_tear_mode
    ap_demo.o(i.ap_get_dcs) refers to ap_demo.o(.data) for flag_te
    ap_demo.o(i.ap_get_finger_flag) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_get_finger_flag) refers to ap_demo.o(.data) for s_finger_flag
    ap_demo.o(i.ap_get_reg_ca) refers to ap_demo.o(.data) for value_reg_ca
    ap_demo.o(i.ap_get_reg_df) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    ap_demo.o(i.ap_get_reg_df) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_get_reg_df) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_get_reg_df) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.ap_get_reg_df) refers to ap_demo.o(.data) for value_reg_df
    ap_demo.o(i.ap_reset_cb) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    ap_demo.o(i.ap_reset_cb) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_reset_cb) refers to hal_system.o(i.hal_system_set_pvd) for hal_system_set_pvd
    ap_demo.o(i.ap_reset_cb) refers to hal_system.o(i.hal_system_set_vcc) for hal_system_set_vcc
    ap_demo.o(i.ap_reset_cb) refers to ap_demo.o(i.__NVIC_SystemReset) for __NVIC_SystemReset
    ap_demo.o(i.ap_reset_cb) refers to ap_demo.o(.conststring) for .conststring
    ap_demo.o(i.ap_reset_high) refers to hal_system.o(i.hal_system_set_pvd) for hal_system_set_pvd
    ap_demo.o(i.ap_reset_high) refers to hal_system.o(i.hal_system_set_vcc) for hal_system_set_vcc
    ap_demo.o(i.ap_reset_high) refers to ap_demo.o(i.__NVIC_SystemReset) for __NVIC_SystemReset
    ap_demo.o(i.ap_reset_low) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    ap_demo.o(i.ap_reset_low) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_reset_low) refers to hal_system.o(i.hal_system_set_vcc) for hal_system_set_vcc
    ap_demo.o(i.ap_reset_low) refers to ap_demo.o(i.ap_reset_high) for ap_reset_high
    ap_demo.o(i.ap_set_backlight) refers to ap_demo.o(.data) for value_reg_b1
    ap_demo.o(i.ap_set_display_off) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_display_off) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_display_off) refers to ap_demo.o(i.finger_calibration_init) for finger_calibration_init
    ap_demo.o(i.ap_set_display_on) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) for hal_dsi_rx_ctrl_set_sw_tear_mode
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to ap_demo.o(i.Gpio_swire_output) for Gpio_swire_output
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin) for hal_dsi_tx_ctrl_panel_reset_pin
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to ap_demo.o(.data) for g_rx_ctrl_handle
    ap_demo.o(i.ap_set_exit_sleep_mode) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_exit_sleep_mode) refers to ap_demo.o(.data) for g_exit_sleep_mode
    ap_demo.o(i.blue_change_ccm) refers to memcpya.o(.text) for __aeabi_memcpy4
    ap_demo.o(i.blue_change_ccm) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) for hal_dsi_tx_ctrl_set_ccm
    ap_demo.o(i.finger_calibration_init) refers to ap_demo.o(.data) for s_finger_calibration
    ap_demo.o(i.finger_calibration_time_counter_exec) refers to tau_delay.o(i.delayUs) for delayUs
    ap_demo.o(i.finger_calibration_time_counter_exec) refers to ap_demo.o(.data) for s_finger_calibration
    ap_demo.o(i.init_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) for hal_dsi_tx_ctrl_create_handle
    ap_demo.o(i.init_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    ap_demo.o(i.init_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) for hal_dsi_tx_ctrl_set_overwrite_rgb
    ap_demo.o(i.init_mipi_tx) refers to ap_demo.o(.data) for g_tx_ctrl_handle
    ap_demo.o(i.init_panel) refers to ap_demo.o(i.tx_panel_reset) for tx_panel_reset
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) for hal_dsi_tx_ctrl_enter_init_panel_mode
    ap_demo.o(i.init_panel) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.init_panel) refers to tau_delay.o(i.delayUs) for delayUs
    ap_demo.o(i.init_panel) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    ap_demo.o(i.init_panel) refers to ap_demo.o(i.soft_te_timer_init) for soft_te_timer_init
    ap_demo.o(i.init_panel) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.init_panel) refers to ap_demo.o(i.Gpio_swire_output) for Gpio_swire_output
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) for hal_dsi_tx_ctrl_exit_init_panel_mode
    ap_demo.o(i.open_mipi_rx) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) for hal_dsi_rx_ctrl_create_handle
    ap_demo.o(i.open_mipi_rx) refers to memcpya.o(.text) for __aeabi_memcpy4
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) for hal_dsi_rx_ctrl_pre_init_pps
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) for hal_dsi_rx_ctrl_set_cus_scld_filter
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(i.blue_change_ccm) for blue_change_ccm
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(.data) for g_rx_ctrl_handle
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(.constdata) for g_cus_rx_dcs_execute_table
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(i.ap_dcs_read) for ap_dcs_read
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(i.pps_update_handle) for pps_update_handle
    ap_demo.o(i.pps_update_handle) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) for hal_dsi_rx_ctrl_toggle_resolution
    ap_demo.o(i.pps_update_handle) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.pps_update_handle) refers to ap_demo.o(.data) for g_rx_ctrl_handle
    ap_demo.o(i.set_soft_tear_mode) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex) for hal_dsi_rx_ctrl_set_tear_mode_ex
    ap_demo.o(i.set_soft_tear_mode) refers to ap_demo.o(.data) for flag_te
    ap_demo.o(i.soft_swire_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    ap_demo.o(i.soft_swire_init) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.soft_swire_init) refers to ap_demo.o(i.soft_swire_start) for soft_swire_start
    ap_demo.o(i.soft_swire_init) refers to hal_timer.o(i.hal_timer_init) for hal_timer_init
    ap_demo.o(i.soft_swire_init) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    ap_demo.o(i.soft_swire_init) refers to ap_demo.o(.data) for g_swire_num
    ap_demo.o(i.soft_swire_init) refers to ap_demo.o(i.soft_swire_timer_callback) for soft_swire_timer_callback
    ap_demo.o(i.soft_swire_start) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    ap_demo.o(i.soft_swire_start) refers to tau_delay.o(i.delayUs) for delayUs
    ap_demo.o(i.soft_swire_timer_callback) refers to ap_demo.o(i.soft_swire_start) for soft_swire_start
    ap_demo.o(i.soft_swire_timer_callback) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    ap_demo.o(i.soft_swire_timer_callback) refers to ap_demo.o(.data) for g_swire_num
    ap_demo.o(i.soft_te_timer_cb) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) for hal_dsi_rx_ctrl_gen_a_tear_signal
    ap_demo.o(i.soft_te_timer_cb) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    ap_demo.o(i.soft_te_timer_cb) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) for hal_dsi_rx_ctrl_set_hw_tear_mode
    ap_demo.o(i.soft_te_timer_cb) refers to ap_demo.o(.data) for panel_display_done
    ap_demo.o(i.soft_te_timer_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) for hal_dsi_rx_ctrl_set_sw_tear_mode
    ap_demo.o(i.soft_te_timer_init) refers to hal_timer.o(i.hal_timer_init) for hal_timer_init
    ap_demo.o(i.soft_te_timer_init) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    ap_demo.o(i.soft_te_timer_init) refers to ap_demo.o(.data) for g_rx_ctrl_handle
    ap_demo.o(i.soft_te_timer_init) refers to ap_demo.o(i.soft_te_timer_cb) for soft_te_timer_cb
    ap_demo.o(i.soft_timer3_cb) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    ap_demo.o(i.soft_timer3_cb) refers to app_tp_for_custom_s8.o(.data) for tp_sleep_count
    ap_demo.o(i.soft_timer3_cb) refers to ap_demo.o(.data) for phone_DisplayOFF_count
    ap_demo.o(i.swire_callback) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    ap_demo.o(i.swire_callback) refers to ap_demo.o(i.swire_timer_callback) for swire_timer_callback
    ap_demo.o(i.swire_init) refers to hal_swire.o(i.hal_swire_open) for hal_swire_open
    ap_demo.o(i.swire_init) refers to hal_swire.o(i.hal_swire_init) for hal_swire_init
    ap_demo.o(i.swire_init) refers to hal_swire.o(i.hal_swire_register_callback) for hal_swire_register_callback
    ap_demo.o(i.swire_init) refers to hal_swire.o(i.hal_swire_start) for hal_swire_start
    ap_demo.o(i.swire_init) refers to hal_timer.o(i.hal_timer_init) for hal_timer_init
    ap_demo.o(i.swire_init) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    ap_demo.o(i.swire_init) refers to ap_demo.o(i.swire_callback) for swire_callback
    ap_demo.o(i.swire_init) refers to ap_demo.o(i.swire_timer_callback) for swire_timer_callback
    ap_demo.o(i.swire_timer_callback) refers to hal_swire.o(i.hal_swire_start) for hal_swire_start
    ap_demo.o(i.swire_timer_callback) refers to ap_demo.o(.data) for swire_num
    ap_demo.o(i.tp_heartbeat_exec) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    ap_demo.o(i.tp_heartbeat_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) for ap_tp_st_touch_hardware_reset
    ap_demo.o(i.tp_heartbeat_exec) refers to ap_demo.o(.data) for panel_display_done
    ap_demo.o(i.tx_display_on) refers to ap_demo.o(i.init_panel) for init_panel
    ap_demo.o(i.tx_display_on) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    ap_demo.o(i.tx_display_on) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.tx_display_on) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.tx_display_on) refers to ap_demo.o(.data) for g_tx_ctrl_handle
    ap_demo.o(i.tx_panel_reset) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.tx_panel_reset) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin) for hal_dsi_tx_ctrl_panel_reset_pin
    ap_demo.o(i.tx_panel_reset) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_display_on) for ap_set_display_on
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_display_off) for ap_set_display_off
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_get_51_reg) for ap_get_51_reg
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_get_67_reg) for ap_get_67_reg
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_enter_sleep_mode) for ap_set_enter_sleep_mode
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_exit_sleep_mode) for ap_set_exit_sleep_mode
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_get_dcs) for ap_get_dcs
    ap_demo.o(.constdata) refers to app_tp_st_touch.o(i.ap_set_tp_calibration_04) for ap_set_tp_calibration_04
    app_tp_transfer.o(i.ap_doubleclick) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_transfer.o(i.ap_doubleclick) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.ap_doubleclick) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_transfer.o(i.ap_doubleclick) refers to app_tp_transfer.o(.data) for MI10_PRO_screen_init_data10
    app_tp_transfer.o(i.ap_doubleclick_1) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_transfer.o(i.ap_doubleclick_1) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.ap_doubleclick_1) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_transfer.o(i.ap_doubleclick_1) refers to app_tp_transfer.o(.data) for MI10_PRO_screen_init_data11
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(i.app_tp_transfer_phone) for app_tp_transfer_phone
    app_tp_transfer.o(i.app_tp_init) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(i.app_tp_screen_init) for app_tp_screen_init
    app_tp_transfer.o(i.app_tp_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    app_tp_transfer.o(i.app_tp_init) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_master.o(i.hal_i2c_m_dma_init) for hal_i2c_m_dma_init
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_slave.o(i.hal_i2c_s_init) for hal_i2c_s_init
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_slave.o(i.hal_i2c_s_set_transfer) for hal_i2c_s_set_transfer
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read) for hal_i2c_s_nonblocking_read
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_for_custom_s8.o(.data) for g_phone_output_int_pad
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(i.app_tp_i2cs_callback) for app_tp_i2cs_callback
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(.bss) for s_phone_read_buffer
    app_tp_transfer.o(i.app_tp_m_read) refers to hal_i2c_master.o(i.hal_i2c_m_dma_read) for hal_i2c_m_dma_read
    app_tp_transfer.o(i.app_tp_m_transfer_complate) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.app_tp_m_write) refers to hal_i2c_master.o(i.hal_i2c_m_dma_write) for hal_i2c_m_dma_write
    app_tp_transfer.o(i.app_tp_phone_clear_reset_on) refers to app_tp_transfer.o(.data) for s_phone_reset_flag
    app_tp_transfer.o(i.app_tp_phone_reset_on) refers to app_tp_transfer.o(.data) for s_phone_reset_flag
    app_tp_transfer.o(i.app_tp_s_read) refers to hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read) for hal_i2c_s_nonblocking_read
    app_tp_transfer.o(i.app_tp_s_transfer_complate) refers to hal_i2c_slave.o(i.hal_i2c_s_write_complate) for hal_i2c_s_write_complate
    app_tp_transfer.o(i.app_tp_s_transfer_complate) refers to hal_i2c_slave.o(i.hal_i2c_s_read_complate) for hal_i2c_s_read_complate
    app_tp_transfer.o(i.app_tp_s_write) refers to hal_i2c_slave.o(i.hal_i2c_s_dma_write) for hal_i2c_s_dma_write
    app_tp_transfer.o(i.app_tp_screen_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    app_tp_transfer.o(i.app_tp_screen_init) refers to tau_delay.o(i.delayUs) for delayUs
    app_tp_transfer.o(i.app_tp_screen_init) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_transfer.o(i.app_tp_screen_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_rst_pad
    app_tp_transfer.o(i.app_tp_screen_int_callback) refers to app_tp_transfer.o(.data) for s_screen_int_flag
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to hal_gpio.o(i.hal_gpio_ctrl_eint) for hal_gpio_ctrl_eint
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to hal_gpio.o(i.hal_gpio_init_eint) for hal_gpio_init_eint
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to hal_gpio.o(i.hal_gpio_reg_eint_cb) for hal_gpio_reg_eint_cb
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to app_tp_transfer.o(i.app_tp_screen_int_callback) for app_tp_screen_int_callback
    app_tp_transfer.o(i.app_tp_transfer_phone) refers to app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) for app_tp_phone_analysis_data
    app_tp_transfer.o(i.app_tp_transfer_phone) refers to app_tp_transfer.o(i.app_tp_s_read) for app_tp_s_read
    app_tp_transfer.o(i.app_tp_transfer_phone) refers to app_tp_transfer.o(i.app_tp_s_write) for app_tp_s_write
    app_tp_transfer.o(i.app_tp_transfer_phone) refers to app_tp_transfer.o(.bss) for s_phone_read_buffer
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(i.app_tp_screen_int_init) for app_tp_screen_int_init
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to ap_demo.o(.data) for phone_start_flag
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_for_custom_s8.o(.data) for screen_reg_int_data
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(.bss) for s_screen_read_buffer
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(.data) for MI10_PRO_screen_init_data1
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_transfer_screen_const) for app_tp_transfer_screen_const
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_screen_int_lvl_low) for app_tp_screen_int_lvl_low
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_m_transfer_complate) for app_tp_m_transfer_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_spi_master.o(i.hal_spi_m_clear_rxfifo) for hal_spi_m_clear_rxfifo
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to tau_delay.o(i.delayUs) for delayUs
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event) for ap_tp_st_touch_scan_point_record_event
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_F3) for ap_tp_st_touch_error_handler_F3
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_FF) for ap_tp_st_touch_error_handler_FF
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) for app_tp_screen_analysis_int
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(.data) for s_screen_init_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(.data) for screen_reg_int_data
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(.bss) for s_screen_read_buffer
    app_tp_transfer.o(i.app_tp_transfer_screen_start) refers to app_tp_transfer.o(.data) for s_screen_const_transfer_count
    app_tp_st_touch.o(i.CRC16_2) refers to app_tp_st_touch.o(.constdata) for wCRCTalbeAbs
    app_tp_st_touch.o(i.ap_get_tp_calibration_status_01) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) for hal_dsi_rx_ctrl_send_ack_cmd
    app_tp_st_touch.o(i.ap_get_tp_calibration_status_01) refers to app_tp_st_touch.o(.data) for s_calibration_correct_flag
    app_tp_st_touch.o(i.ap_set_tp_calibration_04) refers to memseta.o(.text) for __aeabi_memclr4
    app_tp_st_touch.o(i.ap_set_tp_calibration_04) refers to printfa.o(i.__0printf) for __2printf
    app_tp_st_touch.o(i.ap_set_tp_calibration_04) refers to app_tp_st_touch.o(i.CRC16_2) for CRC16_2
    app_tp_st_touch.o(i.ap_set_tp_calibration_04) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    app_tp_st_touch.o(i.ap_set_tp_calibration_04) refers to app_tp_st_touch.o(.data) for s_calibration_flag
    app_tp_st_touch.o(i.ap_tp_st_touch_calibration) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_st_touch.o(i.ap_tp_st_touch_calibration) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_st_touch.o(i.ap_tp_st_touch_calibration) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_calibration) refers to app_tp_st_touch.o(.data) for st_touch_tp_tuning_FpnlInit
    app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_F3) refers to app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) for ap_tp_st_touch_hardware_reset
    app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_FF) refers to app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) for ap_tp_st_touch_hardware_reset
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to memseta.o(.text) for __aeabi_memclr4
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to app_tp_st_touch.o(.data) for s_calibration_correct_flag
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to tau_log.o(i.LOG_printf) for LOG_printf
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event) for ap_tp_st_touch_simulate_finger_release_event
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init) for ap_tp_st_touch_scan_point_init
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_rst_pad
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to app_tp_st_touch.o(.data) for st_touch_tp_tuning_clearfifo
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init) refers to app_tp_st_touch.o(.bss) for tp_scan_data
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event) refers to app_tp_st_touch.o(.bss) for tp_scan_data
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec) refers to printfa.o(i.__0printf) for __2printf
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event) for ap_tp_st_touch_simulate_finger_release_event
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init) for ap_tp_st_touch_scan_point_init
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec) refers to app_tp_st_touch.o(.bss) for tp_scan_data
    app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event) refers to app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) for app_tp_screen_analysis_int
    app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event) for ap_tp_st_touch_simulate_finger_release_event
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init) for ap_tp_st_touch_scan_point_init
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to app_tp_st_touch.o(.data) for st_touch_tp_tuning_clkreset
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_calibration) for ap_tp_st_touch_calibration
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) for ap_tp_st_touch_get_calibration_success_mark
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to tau_log.o(i.LOG_printf) for LOG_printf
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to app_tp_st_touch.o(.data) for s_calibration_flag
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_init) for hal_system_init
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_enable_systick) for hal_system_enable_systick
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_init_console) for hal_system_init_console
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_set_phy_calibration) for hal_system_set_phy_calibration
    startup_armcm0.o(RESET) refers to startup_armcm0.o(STACK) for __initial_sp
    startup_armcm0.o(RESET) refers to startup_armcm0.o(.text) for Reset_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.HardFault_Handler) for HardFault_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SysTick_Handler) for SysTick_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.VIDC_IRQn_Handler) for VIDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.LCDC_IRQn_Handler) for LCDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.MIPI_RX_IRQn_Handler) for MIPI_RX_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.MIPI_TX_IRQn_Handler) for MIPI_TX_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.MEMC_IRQn_Handler) for MEMC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.VPRE_IRQn_Handler) for VPRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.FLSCTRL_IRQn_Handler) for FLSCTRL_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.DMA_IRQn_Handler) for DMA_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER0_IRQn_Handler) for TIMER0_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER1_IRQn_Handler) for TIMER1_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER2_IRQn_Handler) for TIMER2_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER3_IRQn_Handler) for TIMER3_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.WDG_IRQn_Handler) for WDG_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.UART_IRQn_Handler) for UART_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.I2C0_IRQn_Handler) for I2C0_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.I2C1_IRQn_Handler) for I2C1_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SPIS_IRQn_Handler) for SPIS_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SPIM_IRQn_Handler) for SPIM_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.ADC_IRQn_Handler) for ADC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.PWMDET_IRQn_Handler) for PWMDET_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SWIRE_IRQn_Handler) for SWIRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.AP_NRESET_IRQn_Handler) for AP_NRESET_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT0_IRQn_Handler) for EXTI_INT0_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT1_IRQn_Handler) for EXTI_INT1_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT2_IRQn_Handler) for EXTI_INT2_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT3_IRQn_Handler) for EXTI_INT3_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT4_IRQn_Handler) for EXTI_INT4_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT5_IRQn_Handler) for EXTI_INT5_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT6_IRQn_Handler) for EXTI_INT6_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT7_IRQn_Handler) for EXTI_INT7_IRQn_Handler
    startup_armcm0.o(.text) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to drv_vidc.o(i.drv_vidc_set_module_enable) for drv_vidc_set_module_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) for hal_internal_vsync_get_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to hal_internal_vsync.o(i.hal_internal_rx_dcs_async_handler) for hal_internal_rx_dcs_async_handler
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to hal_internal_vsync.o(i.hal_internal_rx_dcs_polling) for hal_internal_rx_dcs_polling
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg) for drv_dsi_rx_set_ddi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_crgu.o(i.drv_crgu_set_rxbr_src) for drv_crgu_set_rxbr_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_crgu.o(i.drv_crgu_set_rxbr_div) for drv_crgu_set_rxbr_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg) for drv_dsi_rx_set_ipi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_gen_a_tear_signal) for drv_memc_gen_a_tear_signal
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size) for drv_dsi_rx_get_max_ret_size
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) for hal_dsi_rx_ctrl_init_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_rx) for hal_internal_vsync_init_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) for hal_dsi_rx_ctrl_init_dsi_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) for hal_dsi_rx_ctrl_init_rxbr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps) for drv_dsc_dec_set_u8_pps
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) for hal_dsi_rx_ctrl_init_vidc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) for hal_dsi_rx_ctrl_init_memc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_chip_info.o(i.drv_chip_rx_init_done) for drv_chip_rx_init_done
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_vidc_src) for drv_crgu_set_vidc_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_fb_src) for drv_crgu_set_fb_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_fb_div) for drv_crgu_set_fb_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) for hal_dsi_rx_ctrl_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg) for drv_dsi_rx_set_ctrl_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) for drv_dsi_rx_set_up_phy
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap) for drv_dsi_rx_set_lane_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_inten) for drv_dsi_rx_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt) for drv_dsi_rx_set_resp_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_mode) for drv_memc_set_ltpo_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tear_mode) for hal_internal_vsync_get_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_vsync.o(i.hal_internal_check_video_auto_sync) for hal_internal_check_video_auto_sync
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_fs_en_conditions) for drv_memc_set_fs_en_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_lcdc_st_conditions) for drv_memc_set_lcdc_st_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_vidc_sync_cnt) for drv_memc_set_vidc_sync_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_double_buffer) for drv_memc_set_double_buffer
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_active_height) for drv_memc_set_active_height
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_inten) for drv_memc_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_color_format) for drv_rxbr_set_color_format
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th) for drv_rxbr_set_ltpo_drop_th
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_cfg) for drv_rxbr_set_usr_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_col) for drv_rxbr_set_usr_col
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_row) for drv_rxbr_set_usr_row
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg) for drv_rxbr_hline_rcv_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) for hal_internal_vsync_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_src_parameter) for drv_vidc_set_src_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pentile_swap) for drv_vidc_set_pentile_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_dst_parameter) for drv_vidc_set_dst_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_init_module_enable) for drv_vidc_init_module_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_rotation) for drv_vidc_set_rotation
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_init_get_scld_filter_h) for drv_param_init_get_scld_filter_h
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_init_get_scld_filter_v) for drv_param_init_get_scld_filter_v
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef0) for drv_vidc_set_scld_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef1) for drv_vidc_set_scld_hcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef0) for drv_vidc_set_scld_vcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef1) for drv_vidc_set_scld_vcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_p2r_hinitr) for drv_vidc_set_p2r_hinitr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_p2r_hinitb) for drv_vidc_set_p2r_hinitb
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_p2r_filter_init) for drv_param_p2r_filter_init
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_p2r_hcoef0) for drv_vidc_set_p2r_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_mirror) for drv_vidc_set_mirror
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pu_ctrl) for drv_vidc_set_pu_ctrl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter) for drv_dsc_dec_convert_pps_rc_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_write_cmd_entry) refers to hal_internal_vsync.o(i.hal_internal_vsync_register_write_cmd_entry) for hal_internal_vsync_register_write_cmd_entry
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header) for drv_rxbr_set_ack_pkt_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) for hal_internal_vsync_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef0) for drv_vidc_set_scld_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef1) for drv_vidc_set_scld_hcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef0) for drv_vidc_set_scld_vcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef1) for drv_vidc_set_scld_vcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_param_init.o(i.drv_param_init_set_scld_filter) for drv_param_init_set_scld_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) for hal_internal_vsync_set_sync_line
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg) for drv_rxbr_hline_rcv0_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_dcs_direct_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode) for hal_internal_vsync_set_dcs_direct_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) refers to drv_rxbr.o(i.drv_rxbr_set_cmd_filter) for drv_rxbr_set_cmd_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) for drv_dsi_rx_calc_ipi_tx_delay
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg) for drv_dsi_rx_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format) refers to drv_vidc.o(i.drv_vidc_update_src_format) for drv_vidc_update_src_format
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format) refers to drv_vidc.o(i.drv_vidc_set_pentile_swap) for drv_vidc_set_pentile_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dflti.o(.text) for __aeabi_i2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dmul.o(.text) for __aeabi_dmul
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to ddiv.o(.text) for __aeabi_ddiv
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to dflti.o(.text) for __aeabi_i2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to dmul.o(.text) for __aeabi_dmul
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to ddiv.o(.text) for __aeabi_ddiv
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) for hal_dsi_rx_ctrl_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk) for hal_intl_svs_update_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_src) for drv_crgu_set_rxbr_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_div) for drv_crgu_set_rxbr_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_dsco_src) for drv_crgu_set_dsco_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_dsco_src_div) for drv_crgu_set_dsco_src_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_dsc_core_div) for drv_crgu_set_dsc_core_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_te_waveform) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_te_waveform) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_dsi_rx.o(i.drv_dsi_rx_power_up) for drv_dsi_rx_power_up
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) for hal_internal_vsync_toggle_input_frame_rate
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) for hal_internal_sync_input_resolution_change
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution_ex) refers to hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) for hal_internal_sync_input_resolution_change_ex
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution_ex) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fscalb.o(.text) for __ARM_scalbnf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fflti.o(.text) for __aeabi_i2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to ffixi.o(.text) for __aeabi_f2iz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk) for drv_dsi_tx_set_video_chunk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing) for drv_dsi_tx_set_video_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to drv_phy_common.o(i.drv_phy_get_rate_para) for drv_phy_get_rate_para
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to ffixui.o(.text) for __aeabi_f2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to hal_dsi_tx_ctrl.o(.conststring) for .conststring
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) for hal_lcdc_config_upscaler
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to drv_lcdc.o(i.drv_lcdc_config_src_parameter) for drv_lcdc_config_src_parameter
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to hal_internal_vsync.o(i.hal_internal_vsync_update_lcdc_addr) for hal_internal_vsync_update_lcdc_addr
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode_rcv_te) refers to hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) for hal_internal_sync_cmd_mode_rcv_te
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_param_init.o(i.drv_param_init_set_ccm) for drv_param_init_set_ccm
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.constdata) for .constdata
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) for hal_lcdc_config_upscaler
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) for hal_lcdc_config_remains
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_mode_init) for hal_dsi_tx_ctrl_draw_mode_init
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) for hal_dsi_tx_ctrl_set_rect_pixel_data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) for hal_lcdc_config_upscaler
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) for hal_lcdc_config_remains
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_mode_init) for hal_dsi_tx_ctrl_draw_mode_init
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_ulps_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) for drv_dsi_tx_phy_ulps_enter
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_ulps_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) for drv_dsi_tx_phy_ulps_exit
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) for hal_dsi_tx_ctrl_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_tx) for hal_internal_vsync_init_tx
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate) for hal_dsi_tx_config_params_for_lane_rate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) for hal_dsi_tx_count_lane_rate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) for hal_dsi_tx_init_phy_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) for drv_dsi_tx_phy_test_setup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) for hal_lcdc_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) for hal_lcdc_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) for hal_dsi_tx_init_dpi_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) for hal_dsi_tx_init_data_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) for hal_dsi_tx_init_remains
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt) for hal_dsi_tx_init_interrupt
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready) for drv_dsi_tx_phy_status_ready
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload) for drv_dsi_tx_command_get_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) refers to drv_param_init.o(i.drv_param_init_set_ccm) for drv_param_init_set_ccm
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_pq_filter) refers to drv_lcdc.o(i.drv_lcdc_config_scale_up_coef) for drv_lcdc_config_scale_up_coef
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_pq_filter) refers to drv_param_init.o(i.drv_param_init_set_sclu_filter) for drv_param_init_set_sclu_filter
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness) refers to drv_lcdc.o(i.drv_lcdc_config_endianness) for drv_lcdc_config_endianness
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_lp_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd) for drv_dsi_tx_video_mode_set_lp_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb) for drv_lcdc_config_overwrite_rgb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp) refers to drv_lcdc.o(i.drv_lcdc_config_partial_display_enable) for drv_lcdc_config_partial_display_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area) refers to drv_lcdc.o(i.drv_lcdc_config_partial_display_area) for drv_lcdc_config_partial_display_area
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to dflti.o(.text) for __aeabi_i2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to dmul.o(.text) for __aeabi_dmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to ddiv.o(.text) for __aeabi_ddiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_vpg) for drv_dsi_tx_set_vpg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) for hal_dsi_tx_ctrl_draw_flicker
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) for hal_dsi_tx_ctrl_draw_chessboard
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_enable_shadow_reg) for drv_lcdc_enable_shadow_reg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_check_video_auto_sync) for hal_internal_check_video_auto_sync
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_start) for drv_lcdc_start
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_set_video_hw_mode) for drv_lcdc_set_video_hw_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size) for drv_dsi_tx_edpi_cmd_size
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) for hal_dsi_tx_init_video_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode) for drv_dsi_tx_dpi_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity) for drv_dsi_tx_dpi_polarity
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time) for drv_dsi_tx_dpi_lpcmd_time
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_int) for drv_dsi_tx_config_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode) for drv_dsi_tx_phy_lane_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg) for drv_dsi_tx_phy_time_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_response_mode) for drv_dsi_tx_response_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div) for drv_dsi_tx_set_time_out_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg) for drv_dsi_tx_timeout_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp) for drv_dsi_tx_phy_clock_lane_auto_lp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg) for drv_dsi_tx_video_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack) for drv_dsi_tx_set_bta_ack
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd) for drv_dsi_tx_video_mode_set_lp_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_disable_hact_cmd) for drv_dsi_tx_video_mode_disable_hact_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) for hal_dsi_tx_calc_video_chunks
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_header) for drv_dsi_tx_command_header
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) refers to drv_param_init.o(i.drv_param_init_get_ccm) for drv_param_init_get_ccm
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) refers to drv_lcdc.o(i.drv_lcdc_config_ccm) for drv_lcdc_config_ccm
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to hal_internal_vsync.o(i.hal_internal_check_video_auto_sync) for hal_internal_check_video_auto_sync
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_disp_mode) for drv_lcdc_config_disp_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_edpi_mode) for drv_lcdc_config_edpi_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_endianness) for drv_lcdc_config_endianness
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_thresh) for drv_lcdc_config_thresh
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_dpi_polarity) for drv_lcdc_config_dpi_polarity
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_src_parameter) for drv_lcdc_config_src_parameter
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area) for hal_dsi_tx_ctrl_set_partial_disp_area
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp) for hal_dsi_tx_ctrl_set_partial_disp
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_lcdc.o(i.drv_lcdc_config_scale_up_step) for drv_lcdc_config_scale_up_step
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_param_init.o(i.drv_param_init_get_sclu_filter) for drv_param_init_get_sclu_filter
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_lcdc.o(i.drv_lcdc_config_scale_up_coef) for drv_lcdc_config_scale_up_coef
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) for hal_lcdc_config_upscaler
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) for hal_lcdc_config_ccm
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile) for hal_lcdc_config_rgb_to_pentile
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) for hal_lcdc_config_remains
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) for hal_lcdc_init_interrupt
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to drv_lcdc.o(i.drv_lcdc_set_prefetch) for drv_lcdc_set_prefetch
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dpi_pre_div) for drv_crgu_set_dpi_pre_div
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dpi_pre_src) for drv_crgu_set_dpi_pre_src
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dpi_mux_src) for drv_crgu_set_dpi_mux_src
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_lcdc.o(i.drv_lcdc_config_dpi_timing) for drv_lcdc_config_dpi_timing
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to hal_internal_vsync.o(i.hal_internal_check_video_auto_sync) for hal_internal_check_video_auto_sync
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to hal_internal_soft_sync.o(i.hal_intl_svs_init_tx) for hal_intl_svs_init_tx
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to cfrcmple.o(.text) for __aeabi_cfrcmple
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ffixi.o(.text) for __aeabi_f2iz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_lcdc_div) for drv_crgu_set_lcdc_div
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_lcdc_src) for drv_crgu_set_lcdc_src
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) for hal_tx_frame_rate_adjust
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to drv_lcdc.o(i.drv_lcdc_ctrl_flow) for drv_lcdc_ctrl_flow
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to drv_lcdc.o(i.drv_lcdc_config_int) for drv_lcdc_config_int
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to cfcmple.o(.text) for __aeabi_cfcmple
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_gpio.o(i.hal_gpio_ctrl_eint) refers to drv_gpio.o(i.drv_gpio_set_int) for drv_gpio_set_int
    hal_gpio.o(i.hal_gpio_ctrl_eint) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_get_input_data) refers to drv_gpio.o(i.drv_gpio_get_input_data) for drv_gpio_get_input_data
    hal_gpio.o(i.hal_gpio_get_int_type) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to drv_gpio.o(i.drv_gpio_get_pull_state) for drv_gpio_get_pull_state
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_eint) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group) for drv_sys_cfg_sel_gpio_group
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig) for drv_sys_cfg_sel_int_trig
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_init_eint) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_input) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_input) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_input) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_init_output) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_reg_eint_cb) refers to drv_gpio.o(i.drv_gpio_register_callback) for drv_gpio_register_callback
    hal_gpio.o(i.hal_gpio_reg_eint_cb) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_gpio.o(i.drv_gpio_register_ap_reset_callback) for drv_gpio_register_ap_reset_callback
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) for drv_sys_cfg_sel_ap_rst_trig
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to drv_gpio.o(i.drv_gpio_set_driving_strength) for drv_gpio_set_driving_strength
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode3) for drv_gpio_set_mode3
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode2) for drv_gpio_set_mode2
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode1) for drv_gpio_set_mode1
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode0) for drv_gpio_set_mode0
    hal_gpio.o(i.hal_gpio_set_mode) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_output_data) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to drv_gpio.o(i.drv_gpio_set_pull_state) for drv_gpio_set_pull_state
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to drv_gpio.o(i.drv_gpio_set_schmitt_trigger) for drv_gpio_set_schmitt_trigger
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to drv_gpio.o(i.drv_gpio_set_slew_rate) for drv_gpio_set_slew_rate
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to hal_gpio.o(.constdata) for .constdata
    hal_i2c_master.o(i.hal_i2c_m_deinit) refers to drv_i2c_master.o(i.drv_i2c_m_deinit) for drv_i2c_m_deinit
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_master.o(i.drv_i2c_master_init) for drv_i2c_master_init
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_master.o(i.drv_i2c1_set_callback) for drv_i2c1_set_callback
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_master.o(i.drv_i2c_m_enable_intr) for drv_i2c_m_enable_intr
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_dma.o(i.drv_i2c_dma_init) for drv_i2c_dma_init
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_dma.o(i.drv_i2c_enable_rx_dma) for drv_i2c_enable_rx_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_dma.o(i.drv_i2c_enable_tx_dma) for drv_i2c_enable_tx_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to hal_i2c_master.o(i.hal_i2c_master_irq_callback) for hal_i2c_master_irq_callback
    hal_i2c_master.o(i.hal_i2c_m_dma_read) refers to drv_i2c_dma.o(i.drv_i2c_master_read_dma) for drv_i2c_master_read_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_read) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_master.o(i.hal_i2c_m_dma_write) refers to drv_i2c_dma.o(i.drv_i2c_master_write_dma) for drv_i2c_master_write_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_write) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_master.o(i.hal_i2c_m_set_high_impedance) refers to drv_i2c_master.o(i.drv_i2c_m_enable) for drv_i2c_m_enable
    hal_i2c_master.o(i.hal_i2c_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_master.o(i.hal_i2c_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_i2c_master.o(i.hal_i2c_m_transfer_complate) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_master.o(i.hal_i2c_master_irq_callback) refers to drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit) for drv_i2c_m_clear_it_pending_bit
    hal_i2c_master.o(i.hal_i2c_master_irq_callback) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to drv_i2c_slave.o(i.drv_i2c_s_set_intr) for drv_i2c_s_set_intr
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to drv_i2c_slave.o(i.drv_i2c_s_enable) for drv_i2c_s_enable
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to drv_i2c_dma.o(i.drv_i2c_slave_write_dma) for drv_i2c_slave_write_dma
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_get_tx_byte_num) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c_slave_init) for drv_i2c_slave_init
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_master.o(i.drv_i2c1_set_callback) for drv_i2c1_set_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c_s_config_intr) for drv_i2c_s_config_intr
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c_s_set_intr) for drv_i2c_s_set_intr
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_dma.o(i.drv_i2c_dma_init) for drv_i2c_dma_init
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) for drv_i2c_set_dma_irq_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_dma.o(i.drv_i2c_enable_tx_dma) for drv_i2c_enable_tx_dma
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c0_set_callback) for drv_i2c0_set_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) for hal_i2c_slave_irq_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback) for hal_i2c_s_dma_user_callback
    hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_complate) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_complate_clear) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_data) refers to drv_i2c_slave.o(i.drv_i2c_s_read_data) for drv_i2c_s_read_data
    hal_i2c_slave.o(i.hal_i2c_s_read_data) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_data) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_rxfifo_notempty) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    hal_i2c_slave.o(i.hal_i2c_s_rxfifo_notempty) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_rxfifo_notempty) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_sel) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_set_dma_tx_cycle) refers to drv_dma.o(i.drv_dma_enable_cycle) for drv_dma_enable_cycle
    hal_i2c_slave.o(i.hal_i2c_s_set_dma_tx_cycle) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_set_dma_tx_cycle) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to drv_i2c_slave.o(i.drv_i2c_s_enable) for drv_i2c_s_enable
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_set_transfer) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_write_complate) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_write_data) refers to drv_i2c_slave.o(i.drv_i2c_s_write_data) for drv_i2c_s_write_data
    hal_i2c_slave.o(i.hal_i2c_s_write_data) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_write_data) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit) for drv_i2c_s_clear_it_pending_bit
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(i.drv_i2c_s_write_data) for drv_i2c_s_write_data
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_spi_master.o(i.hal_spi_m_callback) refers to drv_spi_dma.o(i.drv_spi_abort_dma) for drv_spi_abort_dma
    hal_spi_master.o(i.hal_spi_m_callback) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_clear_rxfifo) refers to drv_spi_master.o(i.drv_spi_m_read_data) for drv_spi_m_read_data
    hal_spi_master.o(i.hal_spi_m_deinit) refers to drv_spi_master.o(i.drv_spi_m_deinit) for drv_spi_m_deinit
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to hal_spi_master.o(i.hal_spi_m_gpio_init) for hal_spi_m_gpio_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_master.o(i.drv_spi_master_init) for drv_spi_master_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_dma_init) for drv_spi_dma_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_dma_ch6_init) for drv_spi_dma_ch6_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) for drv_spi_set_dma_irq_callback
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) for drv_spi_set_dma_ch6_irq_callback
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req) for drv_sys_cfg_set_dma_rx_req
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_master.o(i.drv_spi_m_enable_rx_dma) for drv_spi_m_enable_rx_dma
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to hal_spi_master.o(i.hal_spi_m_callback) for hal_spi_m_callback
    hal_spi_master.o(i.hal_spi_m_dma_read) refers to drv_spi_dma.o(i.drv_spim_dma_read) for drv_spim_dma_read
    hal_spi_master.o(i.hal_spi_m_dma_read) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_dma_write) refers to drv_spi_dma.o(i.drv_spim_dma_write) for drv_spim_dma_write
    hal_spi_master.o(i.hal_spi_m_dma_write) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_get_transfer_complate) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_gpio_init) refers to drv_spi_master.o(i.drv_spi_m_gpio_init) for drv_spi_m_gpio_init
    hal_spi_master.o(i.hal_spi_m_read_rxfifo) refers to drv_spi_master.o(i.drv_spi_m_read_data) for drv_spi_m_read_data
    hal_spi_master.o(i.hal_spi_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_spi_master.o(i.hal_spi_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    hal_spi_master.o(i.hal_spi_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_swire.o(i.hal_swire_deinit) refers to drv_swire.o(i.drv_swire_enable) for drv_swire_enable
    hal_swire.o(i.hal_swire_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_swire.o(i.hal_swire_init) refers to drv_crgu.o(i.drv_crgu_set_swire_div) for drv_crgu_set_swire_div
    hal_swire.o(i.hal_swire_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_swire.o(i.hal_swire_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_swire.o(i.hal_swire_init) refers to drv_swire.o(i.drv_swire_enable) for drv_swire_enable
    hal_swire.o(i.hal_swire_open) refers to drv_swire.o(i.drv_swire_set_power_down) for drv_swire_set_power_down
    hal_swire.o(i.hal_swire_register_callback) refers to drv_swire.o(i.drv_swire_register_callback) for drv_swire_register_callback
    hal_swire.o(i.hal_swire_start) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    hal_swire.o(i.hal_swire_start) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_swire.o(i.hal_swire_start) refers to drv_swire.o(i.drv_swire_set_bit_time) for drv_swire_set_bit_time
    hal_swire.o(i.hal_swire_start) refers to drv_swire.o(i.drv_swire_set_pulse_count) for drv_swire_set_pulse_count
    hal_swire.o(i.hal_swire_start) refers to drv_common.o(.data) for g_system_clock
    hal_system.o(i.hal_system_deep_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode) for drv_pwr_enter_deep_sleep_mode
    hal_system.o(i.hal_system_disable_systick) refers to drv_common.o(i.drv_common_disable_systick) for drv_common_disable_systick
    hal_system.o(i.hal_system_enable_systick) refers to drv_common.o(i.drv_common_enable_systick) for drv_common_enable_systick
    hal_system.o(i.hal_system_get_tick) refers to drv_common.o(i.drv_common_get_tick) for drv_common_get_tick
    hal_system.o(i.hal_system_idle_mode) refers to drv_common.o(i.drv_common_idle_mode) for drv_common_idle_mode
    hal_system.o(i.hal_system_init) refers to drv_pwr.o(i.drv_pwr_set_system_clk_src) for drv_pwr_set_system_clk_src
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_set_ahb_src) for drv_crgu_set_ahb_src
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_set_ahb_pre_div) for drv_crgu_set_ahb_pre_div
    hal_system.o(i.hal_system_init) refers to irq_redirect .o(i.handle_init) for handle_init
    hal_system.o(i.hal_system_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int) for drv_sys_cfg_clear_all_int
    hal_system.o(i.hal_system_init) refers to drv_common.o(i.drv_common_system_init) for drv_common_system_init
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_system.o(i.hal_system_init) refers to drv_pwr.o(i.drv_pwr_set_pvd_mode) for drv_pwr_set_pvd_mode
    hal_system.o(i.hal_system_init) refers to drv_common.o(.data) for g_system_clock
    hal_system.o(i.hal_system_init_console) refers to hal_uart.o(i.hal_uart_init) for hal_uart_init
    hal_system.o(i.hal_system_register_systick_cb) refers to drv_common.o(i.drv_common_systick_register_cb) for drv_common_systick_register_cb
    hal_system.o(i.hal_system_set_phy_calibration) refers to drv_phy_common.o(i.drv_phy_enable_calibration) for drv_phy_enable_calibration
    hal_system.o(i.hal_system_set_pvd) refers to drv_pwr.o(i.drv_pwr_set_pvd_mode) for drv_pwr_set_pvd_mode
    hal_system.o(i.hal_system_set_vcc) refers to drv_pwr.o(i.drv_pwr_set_cp_mode) for drv_pwr_set_cp_mode
    hal_system.o(i.hal_system_share_flash_mode) refers to drv_fls.o(i.drv_fls_gpio_connect) for drv_fls_gpio_connect
    hal_system.o(i.hal_system_share_flash_mode) refers to drv_fls.o(i.drv_fls_gpio_disconnect) for drv_fls_gpio_disconnect
    hal_system.o(i.hal_system_sleep_mode) refers to drv_crgu.o(i.drv_crgu_config_clocks) for drv_crgu_config_clocks
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_set_repeat) for drv_timer_set_repeat
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_timer.o(i.hal_timer_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_timer.o(i.hal_timer_get_status) refers to drv_timer.o(i.drv_timer_get_status) for drv_timer_get_status
    hal_timer.o(i.hal_timer_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_timer.o(i.hal_timer_init) refers to drv_timer.o(i.drv_timer_set_prescaler) for drv_timer_set_prescaler
    hal_timer.o(i.hal_timer_set_repeat) refers to drv_timer.o(i.drv_timer_set_repeat) for drv_timer_set_repeat
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_get_prescaler) for drv_timer_get_prescaler
    hal_timer.o(i.hal_timer_start) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_start) refers to drv_common.o(.data) for g_system_clock
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_get_prescaler) for drv_timer_get_prescaler
    hal_timer.o(i.hal_timer_start_ex) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_start_ex) refers to drv_common.o(.data) for g_system_clock
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    tau_delay.o(i.delayMs) refers to tau_delay.o(i.delayUs) for delayUs
    tau_log.o(i.LOG_printf) refers to printfa.o(i.__0vsprintf) for vsprintf
    tau_log.o(i.LOG_printf) refers to printfa.o(i.__0printf) for __2printf
    tau_log.o(i.LOG_printf) refers to tau_log.o(.bss) for .bss
    tau_log.o(i.fgetc) refers to hal_uart.o(i.hal_uart_receive_blocking) for hal_uart_receive_blocking
    tau_log.o(i.fputc) refers to hal_uart.o(i.hal_uart_transmit_blocking) for hal_uart_transmit_blocking
    app_tp_for_custom_s8.o(i.EncryptCheck) refers to app_tp_for_custom_s8.o(.data) for enctryptCnt
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to app_tp_for_custom_s8.o(.data) for sleep_double_EN
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to app_tp_for_custom_s8.o(.constdata) for sleep_on
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to ap_demo.o(.data) for phone_86_flag
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to app_tp_transfer.o(.data) for s_screen_read_MI10Pro
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to app_tp_transfer.o(i.app_tp_screen_init) for app_tp_screen_init
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to tau_log.o(i.LOG_printf) for LOG_printf
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to app_tp_for_custom_s8.o(.data) for app_tp_count
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to app_tp_for_custom_s8.o(i.EncryptCheck) for EncryptCheck
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to app_tp_for_custom_s8.o(.data) for phone_reg_coord_back
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.constdata) for phone_b6_00_28_data
    hal_uart.o(i.hal_uart_deinit) refers to drv_dma.o(i.drv_dma_deinit) for drv_dma_deinit
    hal_uart.o(i.hal_uart_deinit) refers to drv_uart.o(i.UART_Deinit) for UART_Deinit
    hal_uart.o(i.hal_uart_dmacallback) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_uart.o(i.hal_uart_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_uart.o(i.hal_uart_init) refers to drv_uart.o(i.UART_init) for UART_init
    hal_uart.o(i.hal_uart_init) refers to drv_common.o(.data) for g_system_clock
    hal_uart.o(i.hal_uart_init) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_receive_blocking) refers to drv_uart.o(i.UART_ReadBlocking) for UART_ReadBlocking
    hal_uart.o(i.hal_uart_receive_dma) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    hal_uart.o(i.hal_uart_receive_dma) refers to drv_uart_dma.o(i.UART_TransferCreateHandleDMA) for UART_TransferCreateHandleDMA
    hal_uart.o(i.hal_uart_receive_dma) refers to drv_uart_dma.o(i.UART_TransferReceiveDMA) for UART_TransferReceiveDMA
    hal_uart.o(i.hal_uart_receive_dma) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_receive_dma) refers to hal_uart.o(i.hal_uart_dmacallback) for hal_uart_dmacallback
    hal_uart.o(i.hal_uart_transmit_blocking) refers to drv_uart.o(i.UART_WriteBlocking) for UART_WriteBlocking
    hal_uart.o(i.hal_uart_transmit_dma) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    hal_uart.o(i.hal_uart_transmit_dma) refers to drv_uart_dma.o(i.UART_TransferCreateHandleDMA) for UART_TransferCreateHandleDMA
    hal_uart.o(i.hal_uart_transmit_dma) refers to drv_uart_dma.o(i.UART_TransferSendDMA) for UART_TransferSendDMA
    hal_uart.o(i.hal_uart_transmit_dma) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_transmit_dma) refers to hal_uart.o(i.hal_uart_dmacallback) for hal_uart_dmacallback
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_param_init.o(i.drv_param_init_get_ccm) for drv_param_init_get_ccm
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_lcdc.o(i.drv_lcdc_config_ccm) for drv_lcdc_config_ccm
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to ddiv.o(.text) for __aeabi_ddiv
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to sqrt.o(i.sqrt) for sqrt
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to dmul.o(.text) for __aeabi_dmul
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to cdcmple.o(.text) for __aeabi_cdcmple
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to hal_internal_vsync.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_get_pkt_buf_error_status) for drv_rxbr_get_pkt_buf_error_status
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.dcs_sw_filter) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.dcs_sw_filter) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_check_video_auto_sync) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tear_mode) for hal_internal_vsync_get_tear_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_mode) for drv_memc_set_ltpo_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_double_buffer) for drv_memc_set_double_buffer
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_active_height) for drv_memc_set_active_height
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_inten) for drv_memc_set_inten
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_rx_dcs_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) for dcs_packet_get_fifo_header
    hal_internal_vsync.o(i.hal_internal_rx_dcs_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) for dcs_packet_free_fifo_header
    hal_internal_vsync.o(i.hal_internal_rx_dcs_polling) refers to hal_internal_vsync.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_vsync.o(i.hal_internal_rx_dcs_polling) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_bta_status) for drv_dsi_rx_get_bta_status
    hal_internal_vsync.o(i.hal_internal_rx_dcs_polling) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.hal_internal_rx_dcs_polling) refers to hal_internal_vsync.o(i.drv_rxbr_get_status1) for drv_rxbr_get_status1
    hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) refers to drv_lcdc.o(i.drv_lcdc_start) for drv_lcdc_start
    hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) for hal_dsi_rx_ctrl_gen_a_tear_signal
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_delay.o(i.delayUs) for delayUs
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.hal_internal_init_memc) for hal_internal_init_memc
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to drv_lcdc.o(i.drv_lcdc_enable_shadow_reg) for drv_lcdc_enable_shadow_reg
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to tau_delay.o(i.delayMs) for delayMs
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) for hal_dsi_rx_ctrl_gen_a_tear_signal
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to tau_delay.o(i.delayUs) for delayUs
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) for hal_vsync_reset_lcdc_scaler
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_internal_vsync.o(i.vsync_set_te_mode) for vsync_set_te_mode
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_tear_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_chip_info.o(i.drv_chip_rx_info_check) for drv_chip_rx_info_check
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_soft_sync.o(i.hal_intl_svs_init_rx) for hal_intl_svs_init_rx
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_rxbr.o(i.drv_rxbr_register_irq0_callback) for drv_rxbr_register_irq0_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_rxbr.o(i.drv_rxbr_register_irq1_callback) for drv_rxbr_register_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_vidc.o(i.drv_vidc_register_callback) for drv_vidc_register_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_init) for dcs_packet_fifo_init
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_gen_te) for soft_gen_te
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_gen_te_double_buffer) for soft_gen_te_double_buffer
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.rxbr_irq0_callback) for rxbr_irq0_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.rxbr_irq1_callback) for rxbr_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.vidc_callback) for vidc_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_register_write_cmd_entry) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) refers to memseta.o(.text) for __aeabi_memset
    hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) refers to drv_rxbr.o(i.drv_rxbr_set_filter_regs) for drv_rxbr_set_filter_regs
    hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) for hal_internal_vsync_set_auto_hw_filter
    hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_soft_sync.o(i.hal_intl_svs_deinit_tx) for hal_intl_svs_deinit_tx
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_soft_sync.o(i.hal_intl_svs_set_sync_coef) for hal_intl_svs_set_sync_coef
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(i.vsync_set_te_mode) for vsync_set_te_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_soft_sync.o(i.hal_intl_svs_deinit_tx) for hal_intl_svs_deinit_tx
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.vsync_set_te_mode) for vsync_set_te_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_soft_sync.o(i.hal_intl_svs_set_input_frate) for hal_intl_svs_set_input_frate
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg) for drv_rxbr_hline_rcv0_cfg
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_update_lcdc_addr) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dadd.o(.text) for __aeabi_dadd
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area) for hal_dsi_tx_ctrl_set_partial_disp_area
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp) for hal_dsi_tx_ctrl_set_partial_disp
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to drv_param_init.o(i.drv_param_init_get_sclu_filter) for drv_param_init_get_sclu_filter
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to drv_lcdc.o(i.drv_lcdc_config_scale_up_coef) for drv_lcdc_config_scale_up_coef
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_internal_vsync.o(i.hal_internal_init_memc) for hal_internal_init_memc
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(i.dcs_sw_filter) for dcs_sw_filter
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) for dcs_packet_fifo_alloc
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(i.hal_internal_rx_dcs_async_handler) for hal_internal_rx_dcs_async_handler
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_rxbr.o(i.drv_rxbr_get_col_addr) for drv_rxbr_get_col_addr
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_rxbr.o(i.drv_rxbr_get_page_addr) for drv_rxbr_get_page_addr
    hal_internal_vsync.o(i.rx_partial_update) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_dsc_dec.o(i.drv_dsc_dec_get_nslc) for drv_dsc_dec_get_nslc
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_crgu.o(i.drv_crgu_set_dsco_src) for drv_crgu_set_dsco_src
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_crgu.o(i.drv_crgu_set_dsco_src_div) for drv_crgu_set_dsco_src_div
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_crgu.o(i.drv_crgu_set_dsc_core_div) for drv_crgu_set_dsc_core_div
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rx_partial_update) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(i.rx_get_dcs_packet_data) for rx_get_dcs_packet_data
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(i.rx_receive_pps) for rx_receive_pps
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(i.drv_rxbr_get_status1) for drv_rxbr_get_status1
    hal_internal_vsync.o(i.rx_receive_packet) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_bta_status) for drv_dsi_rx_get_bta_status
    hal_internal_vsync.o(i.rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_get_pkt_buf_error_status) for drv_rxbr_get_pkt_buf_error_status
    hal_internal_vsync.o(i.rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_receive_pps) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.rx_receive_pps) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rx_receive_pps) refers to hal_internal_vsync.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter) for drv_dsc_dec_convert_pps_rc_parameter
    hal_internal_vsync.o(i.rx_receive_pps) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps) for drv_dsc_dec_set_u8_pps
    hal_internal_vsync.o(i.rx_receive_pps) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.rx_receive_pps) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_int_source) for drv_rxbr_get_int_source
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.rx_receive_packet) for rx_receive_packet
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.vpre_err_reset) for vpre_err_reset
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.rx_partial_update) for rx_partial_update
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_int_source) for drv_rxbr_get_int_source
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_soft_sync.o(i.hal_intl_svs_handle) for hal_intl_svs_handle
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.vpre_err_reset) for vpre_err_reset
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_lcdc.o(i.drv_lcdc_start) for drv_lcdc_start
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_memc.o(i.drv_memc_set_double_buffer_reverse) for drv_memc_set_double_buffer_reverse
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.soft_gen_te_double_buffer) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_gen_te_double_buffer) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_get_irq_status) for drv_vidc_get_irq_status
    hal_internal_vsync.o(i.vidc_callback) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_internal_vsync.o(i.vidc_callback) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_clear_irq) for drv_vidc_clear_irq
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_internal_vsync.o(i.vidc_callback) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps) for drv_dsc_dec_set_u8_pps
    hal_internal_vsync.o(i.vpre_err_reset) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to drv_lcdc.o(i.drv_lcdc_ctrl_flow) for drv_lcdc_ctrl_flow
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(.data) refers to hal_internal_vsync.o(.bss) for sg_te_info
    drv_common.o(i.app_HardFault_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_common.o(i.app_SysTick_Handler) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_enable_systick) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_common.o(i.drv_common_enable_systick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_get_tick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_system_init) refers to drv_chip_info.o(i.drv_chip_info_init) for drv_chip_info_init
    drv_common.o(i.drv_common_systick_register_cb) refers to drv_common.o(.data) for .data
    drv_dma.o(i.app_dma_irq_handler) refers to drv_dma.o(i.drv_dma_irq_handler) for drv_dma_irq_handler
    drv_dma.o(i.drv_dma_abort_transfer) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_abort_transfer) refers to drv_dma.o(i.drv_dma_disenable_channel_interrupts) for drv_dma_disenable_channel_interrupts
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_disenable_channel_interrupts) for drv_dma_disenable_channel_interrupts
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_clear_flag) for drv_dma_clear_flag
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_set_ccr) for drv_dma_set_ccr
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_dma.o(i.drv_dma_clear_flag) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.drv_dma_create_handle) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dma.o(i.drv_dma_disenable_channel_interrupts) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.drv_dma_enable_channel_interrupts) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dma.o(i.drv_dma_enable_cycle) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_get_remaining_bytes) refers to drv_dma.o(i.drv_dma_channel_is_active) for drv_dma_channel_is_active
    drv_dma.o(i.drv_dma_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dma.o(i.drv_dma_init) refers to drv_dma.o(i.drv_dma_ahb_init) for drv_dma_ahb_init
    drv_dma.o(i.drv_dma_irq_handler) refers to drv_dma.o(i.drv_dma_get_channel_flag) for drv_dma_get_channel_flag
    drv_dma.o(i.drv_dma_irq_handler) refers to drv_dma.o(i.drv_dma_clear_flag) for drv_dma_clear_flag
    drv_dma.o(i.drv_dma_irq_handler) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_m2m_init) refers to memseta.o(.text) for __aeabi_memclr4
    drv_dma.o(i.drv_dma_m2m_init) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    drv_dma.o(i.drv_dma_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_dma.o(i.drv_dma_set_burst) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_set_transfer) refers to drv_dma.o(i.drv_dma_set_burst) for drv_dma_set_burst
    drv_dma.o(i.drv_dma_start_transfer) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    drv_dma.o(i.drv_dma_start_transfer) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_fls.o(i.drv_fls_gpio_connect) refers to drv_fls.o(i.drv_fls_gpio_disconnect) for drv_fls_gpio_disconnect
    drv_fls.o(i.drv_fls_gpio_disconnect) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_EnableClk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_busy_pending) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    drv_fls.o(i.fls_de_init) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    drv_fls.o(i.fls_de_init) refers to drv_dma.o(i.drv_dma_clear_flag) for drv_dma_clear_flag
    drv_fls.o(i.fls_de_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_disable_it) refers to drv_fls.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_fls.o(i.fls_disable_it) refers to drv_fls.o(i.fls_set_mc_irq_mask) for fls_set_mc_irq_mask
    drv_fls.o(i.fls_enable_it) refers to drv_fls.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_fls.o(i.fls_enable_it) refers to drv_fls.o(i.fls_set_mc_irq_mask) for fls_set_mc_irq_mask
    drv_fls.o(i.fls_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_init) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_spi_init) for fls_spi_init
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_ctrl_cfg_init) for fls_ctrl_cfg_init
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_set_tuning) for fls_set_tuning
    drv_fls.o(i.fls_init) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_enable_it) for fls_enable_it
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_set_mc_irq_mask) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_fls.o(i.fls_set_mc_irq_mask) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_set_write) for fls_set_write
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_set_write) for fls_set_write
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect) for drv_ap_rst_trig_edge_detect
    drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_get_pull_state) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_register_ap_reset_callback) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.drv_gpio_register_callback) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_set_driving_strength) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.drv_gpio_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_gpio.o(i.drv_gpio_set_pull_state) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_set_schmitt_trigger) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_set_slew_rate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_i2c_dma.o(i.drv_i2c_dma_callback) refers to drv_i2c_dma.o(.data) for .data
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_i2c_master.o(i.drv_i2c_m_enable) for drv_i2c_m_enable
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req) for drv_sys_cfg_set_dma_rx_req
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_dma.o(i.drv_dma_set_transfer) for drv_dma_set_transfer
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_i2c_dma.o(i.drv_i2c_master_write_read_cmd) for drv_i2c_master_write_read_cmd
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_dma.o(i.drv_dma_set_transfer) for drv_dma_set_transfer
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_i2c_dma.o(.data) for .data
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_i2c_dma.o(.bss) for .bss
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_i2c_dma.o(i.drv_i2c_dma_callback) for drv_i2c_dma_callback
    drv_i2c_dma.o(i.drv_i2c_slave_write_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_i2c_master.o(i.app_I2C1_IRQn_Handler) refers to drv_i2c_master.o(.data) for .data
    drv_i2c_master.o(i.drv_i2c1_set_callback) refers to drv_i2c_master.o(.data) for .data
    drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_deinit) refers to drv_i2c_master.o(i.drv_i2c_m_disable_intr) for drv_i2c_m_disable_intr
    drv_i2c_master.o(i.drv_i2c_m_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_i2c_master.o(i.drv_i2c_m_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_i2c_master.o(i.drv_i2c_m_deinit) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_enable_intr) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_read_data) refers to drv_i2c_master.o(i.drv_i2c_m_get_fifo_status) for drv_i2c_m_get_fifo_status
    drv_i2c_master.o(i.drv_i2c_m_set_sys_mask) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_write_data) refers to drv_i2c_master.o(i.drv_i2c_m_get_fifo_status) for drv_i2c_m_get_fifo_status
    drv_i2c_master.o(i.drv_i2c_master_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_i2c_master.o(i.drv_i2c_master_init) refers to drv_common.o(.data) for g_system_clock
    drv_i2c_slave.o(i.app_I2C0_IRQn_Handler) refers to drv_i2c_slave.o(.data) for .data
    drv_i2c_slave.o(i.drv_i2c0_set_callback) refers to drv_i2c_slave.o(.data) for .data
    drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_i2c_slave.o(i.drv_i2c_s_read_data) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    drv_i2c_slave.o(i.drv_i2c_s_set_intr) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_i2c_slave.o(i.drv_i2c_s_set_intr) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_i2c_slave.o(i.drv_i2c_s_write_data) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    drv_i2c_slave.o(i.drv_i2c_slave_init) refers to drv_i2c_slave.o(i.drv_i2c_s_enable) for drv_i2c_s_enable
    drv_param_init.o(i.drv_param_init_get_ccm) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_get_scld_filter_h) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_get_scld_filter_v) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_get_sclu_filter) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_set_ccm) refers to memcpya.o(.text) for __aeabi_memcpy4
    drv_param_init.o(i.drv_param_init_set_ccm) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_set_scld_filter) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_set_sclu_filter) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_p2r_filter_init) refers to drv_param_init.o(.constdata) for .constdata
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_dma.o(i.drv_dma_disenable_channel_interrupts) for drv_dma_disenable_channel_interrupts
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_master.o(i.drv_spi_m_enable_rx_dma) for drv_spi_m_enable_rx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_slave.o(i.drv_spi_s_enable_tx_dma) for drv_spi_s_enable_tx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_slave.o(i.drv_spi_s_enable_rx_dma) for drv_spi_s_enable_rx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_dma.o(i.drv_spi_dma_callback) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_dma_ch6_init) refers to drv_spi_dma.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_dma.o(i.drv_spi_dma_ch6_init) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_dma_init) refers to drv_spi_dma.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_dma.o(i.drv_spi_dma_init) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_spi_dma.o(i.drv_spi_dma_callback) for drv_spi_dma_callback
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_spi_dma.o(i.drv_spi_dma_callback) for drv_spi_dma_callback
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_spi_master.o(i.drv_spi_m_enable_rx_dma) for drv_spi_m_enable_rx_dma
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_spi_slave.o(i.drv_spi_s_enable_tx_dma) for drv_spi_s_enable_tx_dma
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_master.o(i.app_SPIM_IRQn_Handler) refers to drv_spi_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_master.o(i.app_SPIM_IRQn_Handler) refers to drv_spi_master.o(.data) for .data
    drv_spi_master.o(i.drv_spi_m_deinit) refers to drv_spi_master.o(i.drv_spi_m_switch_sclk) for drv_spi_m_switch_sclk
    drv_spi_master.o(i.drv_spi_m_disable_int) refers to drv_spi_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_master.o(i.drv_spi_m_set_intr_callback) refers to drv_spi_master.o(.data) for .data
    drv_spi_master.o(i.drv_spi_master_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_spi_master.o(i.drv_spi_master_init) refers to drv_common.o(.data) for g_system_clock
    drv_swire.o(i.app_SWIRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_swire.o(i.app_SWIRE_IRQn_Handler) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    drv_swire.o(i.app_SWIRE_IRQn_Handler) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_register_callback) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_swire.o(i.drv_swire_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig) for drv_sys_cfg_sel_ap_rst_lvl_trig
    drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect) refers to drv_sys_cfg.o(.data) for .data
    drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig) for drv_sys_cfg_sel_ap_rst_lvl_trig
    drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) refers to drv_sys_cfg.o(.data) for .data
    drv_timer.o(i.app_TIMER0_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.app_TIMER1_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.app_TIMER2_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.app_TIMER3_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_timer.o(i.drv_timer_enable) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_get_instance) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_get_prescaler) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_get_status) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_clear_status_flags) for drv_timer_clear_status_flags
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_register_callback) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_compare_val) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_timer.o(i.drv_timer_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_repeat) refers to drv_timer.o(.data) for .data
    hal_internal_soft_sync.o(i.hal_intl_svs_deinit_rx) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_soft_sync.o(i.hal_intl_svs_deinit_rx) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.hal_intl_svs_deinit_rx) refers to hal_internal_soft_sync.o(i.svs_wait_start) for svs_wait_start
    hal_internal_soft_sync.o(i.hal_intl_svs_deinit_tx) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.hal_intl_svs_handle) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.hal_intl_svs_init_rx) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_soft_sync.o(i.hal_intl_svs_init_rx) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_soft_sync.o(i.hal_intl_svs_init_rx) refers to hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk) for hal_intl_svs_update_rxbr_clk
    hal_internal_soft_sync.o(i.hal_intl_svs_init_rx) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.hal_intl_svs_init_rx) refers to hal_internal_soft_sync.o(i.svs_wait_start) for svs_wait_start
    hal_internal_soft_sync.o(i.hal_intl_svs_init_tx) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.hal_intl_svs_set_input_frate) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_soft_sync.o(i.hal_intl_svs_set_input_frate) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_soft_sync.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_soft_sync.o(i.svs_wait_start) for svs_wait_start
    hal_internal_soft_sync.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_soft_sync.o(i.svs_waite_fr_stab) for svs_waite_fr_stab
    hal_internal_soft_sync.o(i.hal_intl_svs_set_sync_coef) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk) refers to dmul.o(.text) for __aeabi_dmul
    hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.svs_direct_mode_setting) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_soft_sync.o(i.svs_direct_mode_setting) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_internal_soft_sync.o(i.svs_direct_mode_setting) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_soft_sync.o(i.svs_direct_mode_setting) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg) for drv_rxbr_hline_rcv1_cfg
    hal_internal_soft_sync.o(i.svs_direct_mode_setting) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.svs_get_rel_intv) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_soft_sync.o(i.svs_get_rel_intv) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to hal_internal_soft_sync.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to f2d.o(.text) for __aeabi_f2d
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to dadd.o(.text) for __aeabi_dadd
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.svs_wait_start) refers to hal_internal_soft_sync.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_soft_sync.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_internal_soft_sync.o(i.svs_wait_start) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_soft_sync.o(i.svs_wait_start) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_soft_sync.o(i.svs_wait_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_internal_soft_sync.o(i.svs_wait_start) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_soft_sync.o(i.svs_wait_start) refers to f2d.o(.text) for __aeabi_f2d
    hal_internal_soft_sync.o(i.svs_wait_start) refers to ceil.o(i.ceil) for ceil
    hal_internal_soft_sync.o(i.svs_wait_start) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_soft_sync.o(i.svs_wait_start) refers to hal_internal_soft_sync.o(i.svs_direct_mode_setting) for svs_direct_mode_setting
    hal_internal_soft_sync.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg) for drv_rxbr_hline_rcv1_cfg
    hal_internal_soft_sync.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_soft_sync.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_soft_sync.o(i.svs_wait_start) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_soft_sync.o(i.svs_wait_start) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.svs_wait_start) refers to hal_internal_soft_sync.o(i.svs_waite_fr_stab) for svs_waite_fr_stab
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to hal_internal_soft_sync.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to ffixui.o(.text) for __aeabi_f2uiz
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to hal_internal_soft_sync.o(i.svs_sync_handle) for svs_sync_handle
    drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to ffltui.o(.text) for __aeabi_ui2f
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fdiv.o(.text) for __aeabi_fdiv
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fmul.o(.text) for __aeabi_fmul
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) for drv_dsi_rx_get_color_bpp
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc) for drv_dsi_rx_get_color_pcc
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fadd.o(.text) for __aeabi_fadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to cfrcmple.o(.text) for __aeabi_cfrcmple
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to f2d.o(.text) for __aeabi_f2d
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dadd.o(.text) for __aeabi_dadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dfixui.o(.text) for __aeabi_d2uiz
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte) for drv_rx_phy_test_write_1_byte
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to drv_dsi_rx.o(i.drv_rx_phy_test_read) for drv_rx_phy_test_read
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap) refers to drv_chip_info.o(i.drv_chip_info_get_info) for drv_chip_info_get_info
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_get_rate_para) for drv_phy_get_rate_para
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_get_calibration) for drv_phy_get_calibration
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_clear) for drv_rx_phy_test_clear
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte) for drv_rx_phy_test_write_1_byte
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte) for drv_rx_phy_test_write_2_byte
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_chip_info.o(i.drv_chip_info_get_info) for drv_chip_info_get_info
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_lock) for drv_rx_phy_test_lock
    drv_dsi_rx.o(i.drv_rx_phy_test_clear) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_rx.o(i.drv_rx_phy_test_lock) refers to drv_phy_common.o(i.drv_phy_test_lock) for drv_phy_test_lock
    drv_dsi_rx.o(i.drv_rx_phy_test_read) refers to drv_phy_common.o(i.drv_phy_test_read) for drv_phy_test_read
    drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_1_byte) for drv_phy_test_write_1_byte
    drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_2_byte) for drv_phy_test_write_2_byte
    drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) for drv_tx_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to drv_dsi_tx.o(i.drv_tx_phy_test_read) for drv_tx_phy_test_read
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_get_rate_para) for drv_phy_get_rate_para
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_get_pll_para) for drv_phy_get_pll_para
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_get_calibration) for drv_phy_get_calibration
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_enter) for drv_tx_phy_test_enter
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_crgu.o(i.drv_crgu_set_mipi_ref_src) for drv_crgu_set_mipi_ref_src
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_crgu.o(i.drv_crgu_set_mipi_cfg_src) for drv_crgu_set_mipi_cfg_src
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_clear) for drv_tx_phy_test_clear
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) for drv_tx_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte) for drv_tx_phy_test_write_2_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_code) for drv_tx_phy_test_write_code
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_exit) for drv_tx_phy_test_exit
    drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) for drv_tx_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_version) for drv_dsi_tx_version
    drv_dsi_tx.o(i.drv_dsi_tx_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_tx.o(i.drv_dsi_tx_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dsi_tx.o(i.drv_tx_phy_test_clear) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_tx.o(i.drv_tx_phy_test_read) refers to drv_phy_common.o(i.drv_phy_test_read) for drv_phy_test_read
    drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_1_byte) for drv_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_2_byte) for drv_phy_test_write_2_byte
    drv_dsi_tx.o(i.drv_tx_phy_test_write_code) refers to drv_phy_common.o(i.drv_phy_test_write_code) for drv_phy_test_write_code
    drv_lcdc.o(i.drv_lcdc_config_src_parameter) refers to drv_lcdc.o(i.drv_lcdc_config_input_size) for drv_lcdc_config_input_size
    drv_lcdc.o(i.drv_lcdc_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_lcdc.o(i.drv_lcdc_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_memc.o(i.app_MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_get_status) for drv_memc_get_status
    drv_memc.o(i.app_MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_clear_status) for drv_memc_clear_status
    drv_memc.o(i.app_MEMC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_rxbr.o(i.app_ADC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.app_ADC_IRQn_Handler) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.app_VPRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.app_VPRE_IRQn_Handler) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_EnableIRQ) for __NVIC_EnableIRQ
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_rxbr.o(i.drv_rxbr_register_irq0_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_register_irq1_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_set_cmd_filter) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_rxbr.o(i.drv_rxbr_soft_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_vidc.o(i.app_VIDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.app_VIDC_IRQn_Handler) refers to drv_vidc.o(.data) for .data
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_vidc.o(i.drv_vidc_register_callback) refers to drv_vidc.o(.data) for .data
    irq_redirect .o(i.ADC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.AP_NRESET_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.DMA_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT0_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT1_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT2_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT3_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT4_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT5_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT6_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT7_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.FLSCTRL_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.HardFault_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.I2C0_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.I2C1_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.LCDC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.MEMC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.MIPI_RX_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.MIPI_TX_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.PWMDET_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SPIM_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SPIS_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SWIRE_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SysTick_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER0_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER1_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER2_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER3_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.UART_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.VIDC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.VPRE_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.WDG_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.handle_init) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.handle_init) refers to drv_common.o(i.app_SysTick_Handler) for app_SysTick_Handler
    irq_redirect .o(i.handle_init) refers to hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) for app_LCDC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler) for app_MIPI_RX_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler) for app_MIPI_TX_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_dma.o(i.app_dma_irq_handler) for app_dma_irq_handler
    irq_redirect .o(i.handle_init) refers to norflash.o(i.app_fls_ctrl_Handler) for app_fls_ctrl_Handler
    irq_redirect .o(i.handle_init) refers to drv_i2c_slave.o(i.app_I2C0_IRQn_Handler) for app_I2C0_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_i2c_master.o(i.app_I2C1_IRQn_Handler) for app_I2C1_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to hal_spi_slave.o(i.app_SPIS_IRQn_Handler) for app_SPIS_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_spi_master.o(i.app_SPIM_IRQn_Handler) for app_SPIM_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_rxbr.o(i.app_VPRE_IRQn_Handler) for app_VPRE_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_rxbr.o(i.app_ADC_IRQn_Handler) for app_ADC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_vidc.o(i.app_VIDC_IRQn_Handler) for app_VIDC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_memc.o(i.app_MEMC_IRQn_Handler) for app_MEMC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER0_IRQn_Handler) for app_TIMER0_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER1_IRQn_Handler) for app_TIMER1_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER2_IRQn_Handler) for app_TIMER2_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER3_IRQn_Handler) for app_TIMER3_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_wdg.o(i.app_WDG_IRQn_Handler) for app_WDG_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_uart.o(i.app_UART_IRQn_Handler) for app_UART_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_pwm.o(i.app_PWMDET_IRQn_Handler) for app_PWMDET_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_swire.o(i.app_SWIRE_IRQn_Handler) for app_SWIRE_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) for app_AP_NRESET_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler) for app_EXTI_INT0_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler) for app_EXTI_INT1_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler) for app_EXTI_INT2_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler) for app_EXTI_INT3_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler) for app_EXTI_INT4_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler) for app_EXTI_INT5_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler) for app_EXTI_INT6_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler) for app_EXTI_INT7_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_common.o(i.app_HardFault_Handler) for app_HardFault_Handler
    drv_efuse.o(i.drv_efuse_enter_inactive) refers to drv_efuse.o(i.drv_efuse_int_enable) for drv_efuse_int_enable
    drv_efuse.o(i.drv_efuse_read) refers to drv_efuse.o(i.drv_efuse_read_req) for drv_efuse_read_req
    drv_efuse.o(i.drv_efuse_write) refers to drv_efuse.o(i.drv_efuse_write_req) for drv_efuse_write_req
    drv_phy_common.o(i.drv_phy_enable_calibration) refers to drv_phy_common.o(.data) for .data
    drv_phy_common.o(i.drv_phy_get_calibration) refers to drv_chip_info.o(i.drv_chip_info_get_info) for drv_chip_info_get_info
    drv_phy_common.o(i.drv_phy_get_calibration) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_phy_common.o(i.drv_phy_get_calibration) refers to drv_phy_common.o(.data) for .data
    drv_phy_common.o(i.drv_phy_get_pll_para) refers to drv_phy_common.o(.constdata) for .constdata
    drv_phy_common.o(i.drv_phy_get_rate_para) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_phy_common.o(i.drv_phy_get_rate_para) refers to drv_phy_common.o(.constdata) for .constdata
    drv_phy_common.o(i.drv_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_code) for drv_phy_test_write_code
    drv_phy_common.o(i.drv_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_data) for drv_phy_test_write_data
    drv_phy_common.o(i.drv_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_code) for drv_phy_test_write_code
    drv_phy_common.o(i.drv_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_data) for drv_phy_test_write_data
    drv_chip_info.o(i.drv_chip_info_get_info) refers to drv_chip_info.o(.data) for .data
    drv_chip_info.o(i.drv_chip_info_init) refers to drv_efuse.o(i.drv_efuse_enter_inactive) for drv_efuse_enter_inactive
    drv_chip_info.o(i.drv_chip_info_init) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_chip_info.o(i.drv_chip_info_init) refers to drv_chip_info.o(.data) for .data
    drv_chip_info.o(i.drv_chip_rx_info_check) refers to printfa.o(i.__0printf) for __2printf
    drv_chip_info.o(i.drv_chip_rx_info_check) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_chip_info.o(i.drv_chip_rx_info_check) refers to drv_chip_info.o(.data) for .data
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to drv_efuse.o(i.drv_efuse_enter_inactive) for drv_efuse_enter_inactive
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to printfa.o(i.__0printf) for __2printf
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to hal_spi_slave.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_spi_slave.o(i.hal_spi_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    hal_spi_slave.o(i.hal_spi_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_abort) refers to drv_spi_dma.o(i.drv_spi_abort_dma) for drv_spi_abort_dma
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start) refers to drv_dma.o(i.drv_dma_enable_cycle) for drv_dma_enable_cycle
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start) refers to drv_spi_dma.o(i.drv_spis_dma_write) for drv_spis_dma_write
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_deinit) refers to drv_spi_slave.o(i.drv_spi_s_deinit) for drv_spi_s_deinit
    hal_spi_slave.o(i.hal_spi_slave_enable) refers to drv_spi_slave.o(i.drv_spi_s_enable_int) for drv_spi_s_enable_int
    hal_spi_slave.o(i.hal_spi_slave_enable) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_spi_slave.o(i.hal_spi_slave_enable) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_gpio_init) refers to drv_spi_slave.o(i.drv_spi_s_gpio_init) for drv_spi_s_gpio_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to hal_spi_slave.o(i.hal_spi_slave_gpio_init) for hal_spi_slave_gpio_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_slave.o(i.drv_spi_slave_init) for drv_spi_slave_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_dma.o(i.drv_spi_dma_init) for drv_spi_dma_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) for drv_spi_set_dma_irq_callback
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_slave.o(i.drv_spi_s_enable_tx_dma) for drv_spi_s_enable_tx_dma
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    hal_spi_slave.o(i.hal_spi_slave_init) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_read_data) refers to drv_spi_slave.o(i.drv_spi_s_read_data) for drv_spi_s_read_data
    hal_spi_slave.o(i.hal_spi_slave_register_callback) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_reset_tx) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_set_auto_rx_buffer) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_set_auto_tx_buffer) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_write_data) refers to drv_spi_slave.o(i.drv_spi_s_write_data) for drv_spi_s_write_data
    norflash.o(i.app_fls_ctrl_Handler) refers to drv_fls.o(i.fls_clr_interrupt_flag) for fls_clr_interrupt_flag
    norflash.o(i.app_fls_ctrl_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    norflash.o(i.app_fls_ctrl_Handler) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_best_cfg_init) refers to drv_fls.o(i.fls_spi_init) for fls_spi_init
    norflash.o(i.norflash_best_cfg_init) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_check_id) refers to norflash.o(i.norflash_read_id) for norflash_read_id
    norflash.o(i.norflash_check_id) refers to tau_delay.o(i.delayUs) for delayUs
    norflash.o(i.norflash_check_id) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dma_callback) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dma_read) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_transfer_create_handle_dma) for fls_transfer_create_handle_dma
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_dma_read_prepare) for fls_dma_read_prepare
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_transfer_dma) for fls_transfer_dma
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    norflash.o(i.norflash_dma_read) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dma_read) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_dma_read) refers to norflash.o(i.norflash_dma_callback) for norflash_dma_callback
    norflash.o(i.norflash_dma_write) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_transfer_create_handle_dma) for fls_transfer_create_handle_dma
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_switch_fls_spi) for norflash_switch_fls_spi
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_dma_write_prepare) for fls_dma_write_prepare
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_transfer_dma) for fls_transfer_dma
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    norflash.o(i.norflash_dma_write) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_dma_write) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_dma_callback) for norflash_dma_callback
    norflash.o(i.norflash_dma_write) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dual_read) refers to drv_fls.o(i.fls_ddat_enable) for fls_ddat_enable
    norflash.o(i.norflash_dual_read) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_dual_read) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_switch_fls_spi) for norflash_switch_fls_spi
    norflash.o(i.norflash_dual_write) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_dual_write) refers to drv_fls.o(i.fls_ddat_enable) for fls_ddat_enable
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_en4b) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_read_config_reg) for norflash_read_config_reg
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_en_quad) refers to norflash.o(i.norflash_en_quad_check) for norflash_en_quad_check
    norflash.o(i.norflash_en_quad) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_en_quad) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_en_quad) refers to drv_fls.o(i.fls_busy_pending) for fls_busy_pending
    norflash.o(i.norflash_en_quad) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(i.norflash_get_dual_hstatus) for norflash_get_dual_hstatus
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(i.norflash_get_hstatus) for norflash_get_hstatus
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_erase_block) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_erase_block) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_erase_block) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_erase_block) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_erase_chip) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_erase_chip) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_erase_chip) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_erase_sector) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_erase_sector) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_erase_sector) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_erase_sector) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_ex4b) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_read_config_reg) for norflash_read_config_reg
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_exit_quad) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_exit_quad) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_exit_quad) refers to norflash.o(i.norflash_en_quad_check) for norflash_en_quad_check
    norflash.o(i.norflash_exit_quad) refers to drv_fls.o(i.fls_busy_pending) for fls_busy_pending
    norflash.o(i.norflash_exit_quad) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_get_dual_hstatus) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_get_dual_hstatus) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_get_dual_hstatus) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_get_hstatus) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_get_hstatus) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_get_hstatus) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_get_status) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_get_status) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_get_status) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_get_default_spi_config) for fls_get_default_spi_config
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_get_default_fls_config) for fls_get_default_fls_config
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_get_default_tuning) for fls_get_default_tuning
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_init) for fls_init
    norflash.o(i.norflash_init) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_init) refers to drv_fls.o(.data) for g_fls_tuning
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_qdat_enable) for fls_qdat_enable
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_qadr_enable) for fls_qadr_enable
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_qcmd_enable) for fls_qcmd_enable
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_switch_fls_spi) for norflash_switch_fls_spi
    norflash.o(i.norflash_quad_write) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_quad_write) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_read) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_read_config_reg) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_read_id) refers to drv_fls.o(i.fls_read_cmd) for fls_read_cmd
    norflash.o(i.norflash_read_uid) refers to memseta.o(.text) for __aeabi_memclr4
    norflash.o(i.norflash_read_uid) refers to drv_fls.o(i.fls_read_cmd) for fls_read_cmd
    norflash.o(i.norflash_read_uid) refers to memcpya.o(.text) for __aeabi_memcpy
    norflash.o(i.norflash_set_best_cfg) refers to memseta.o(.text) for __aeabi_memclr4
    norflash.o(i.norflash_set_best_read_cfg) refers to norflash.o(i.norflash_en_quad) for norflash_en_quad
    norflash.o(i.norflash_set_best_read_cfg) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_set_best_read_cfg) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_set_best_write_cfg) refers to norflash.o(i.norflash_en_quad) for norflash_en_quad
    norflash.o(i.norflash_set_best_write_cfg) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_set_best_write_cfg) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_ddat_enable) for fls_ddat_enable
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_qdat_enable) for fls_qdat_enable
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_qadr_enable) for fls_qadr_enable
    norflash.o(i.norflash_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_write) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_write_disable) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_write_disable) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write_disable) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_write_disable) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_write_enable) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_write_enable) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write_enable) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_write_enable) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_big_end_enable) for norflash_big_end_enable
    norflash.o(i.norflash_write_endian_scr) refers to drv_fls.o(i.fls_en_scr) for fls_en_scr
    norflash.o(i.norflash_write_endian_scr) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_big_end_clear) for norflash_big_end_clear
    norflash.o(i.norflash_write_endian_scr) refers to drv_fls.o(i.fls_scr_clear) for fls_scr_clear
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    drv_fls_dma.o(i.fls_abort_dma) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_fls_dma.o(i.fls_abort_dma) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls_dma.o(i.fls_dma_enable) for fls_dma_enable
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_set_write) for fls_set_write
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls_dma.o(i.fls_dma_enable) for fls_dma_enable
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls_dma.o(i.fls_read_dmacallback) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to memseta.o(.text) for __aeabi_memclr4
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_fls_dma.o(.data) for .data
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_fls_dma.o(i.fls_read_dmacallback) for fls_read_dmacallback
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_fls_dma.o(i.fls_write_dmacallback) for fls_write_dmacallback
    drv_fls_dma.o(i.fls_transfer_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_fls_dma.o(i.fls_transfer_dma) refers to drv_dma.o(i.drv_dma_start_transfer) for drv_dma_start_transfer
    drv_fls_dma.o(i.fls_transfer_get_receive_count_dma) refers to drv_dma.o(i.drv_dma_get_remaining_bytes) for drv_dma_get_remaining_bytes
    drv_fls_dma.o(i.fls_write_dmacallback) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_pwm.o(i.app_PWMDET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_pwm.o(i.app_PWMDET_IRQn_Handler) refers to drv_pwm.o(.data) for .data
    drv_pwm.o(i.drv_pwm_in_register_callback) refers to drv_pwm.o(.data) for .data
    drv_pwm.o(i.drv_pwm_in_set_sys_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_pwm.o(i.drv_pwm_in_set_sys_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_spi_slave.o(i.drv_spi_s_deinit) refers to drv_spi_slave.o(i.drv_spi_s_switch_sclk) for drv_spi_s_switch_sclk
    drv_uart.o(i.UART0_IRQ_Handle) refers to drv_uart.o(i.UART_TransferHandleIRQ) for UART_TransferHandleIRQ
    drv_uart.o(i.UART0_IRQ_Handle) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_uart.o(i.UART0_IRQ_Handle) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_AbortReceive) refers to drv_uart.o(i.UART_Disable_IT) for UART_Disable_IT
    drv_uart.o(i.UART_AbortReceive) refers to drv_uart.o(i.UART_ResetRxFIFO) for UART_ResetRxFIFO
    drv_uart.o(i.UART_AbortSend) refers to drv_uart.o(i.UART_Disable_IT) for UART_Disable_IT
    drv_uart.o(i.UART_AbortSend) refers to drv_uart.o(i.UART_ResetTxFIFO) for UART_ResetTxFIFO
    drv_uart.o(i.UART_Deinit) refers to drv_uart.o(i.UART_SwitchSCLK) for UART_SwitchSCLK
    drv_uart.o(i.UART_Disable_IT) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_Disable_IT) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.UART_Disable_IT) refers to drv_uart.o(.constdata) for .constdata
    drv_uart.o(i.UART_EnableDma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req) for drv_sys_cfg_set_dma_rx_req
    drv_uart.o(i.UART_EnableDma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    drv_uart.o(i.UART_Enable_IT) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_Enable_IT) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.UART_GetDefaultConfig) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.UART_GetDefaultConfig) refers to drv_common.o(.data) for g_system_clock
    drv_uart.o(i.UART_GetFIFO_Ctrl) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_GetFIFO_Ctrl) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_ResetRxFIFO) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_ResetRxFIFO) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_ResetTxFIFO) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_ResetTxFIFO) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_SetBaudRate) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_uart.o(i.UART_SwitchSCLK) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_uart.o(i.UART_TransferCreateHandle) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_TransferCreateHandle) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.UART_TransferCreateHandle) refers to drv_uart.o(i.UART_Enable_IT) for UART_Enable_IT
    drv_uart.o(i.UART_TransferCreateHandle) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_TransferHandleIRQ) refers to drv_uart.o(i.UART_ResetRxFIFO) for UART_ResetRxFIFO
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_DisableDma) for UART_DisableDma
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_SwitchSCLK) for UART_SwitchSCLK
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_SetBaudRate) for UART_SetBaudRate
    drv_uart.o(i.UART_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.UART_init) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.app_UART_IRQn_Handler) refers to drv_uart.o(i.UART0_IRQ_Handle) for UART0_IRQ_Handle
    drv_uart_dma.o(i.UART_DMAInit) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart_dma.o(i.UART_DMAInit) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    drv_uart_dma.o(i.UART_TransferAbortReceiveDMA) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_uart_dma.o(i.UART_TransferAbortSendDMA) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart.o(i.UART_EnableDma) for UART_EnableDma
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(i.UART_DMAInit) for UART_DMAInit
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(.data) for .data
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(i.UART_TransferReceiveDMACallback) for UART_TransferReceiveDMACallback
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(i.UART_TransferSendDMACallback) for UART_TransferSendDMACallback
    drv_uart_dma.o(i.UART_TransferGetReceiveCountDMA) refers to drv_dma.o(i.drv_dma_get_remaining_bytes) for drv_dma_get_remaining_bytes
    drv_uart_dma.o(i.UART_TransferReceiveDMA) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_uart_dma.o(i.UART_TransferReceiveDMA) refers to drv_uart.o(i.UART_EnableDma) for UART_EnableDma
    drv_uart_dma.o(i.UART_TransferReceiveDMA) refers to drv_dma.o(i.drv_dma_start_transfer) for drv_dma_start_transfer
    drv_uart_dma.o(i.UART_TransferSendDMA) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_uart_dma.o(i.UART_TransferSendDMA) refers to drv_uart.o(i.UART_EnableDma) for UART_EnableDma
    drv_uart_dma.o(i.UART_TransferSendDMA) refers to drv_dma.o(i.drv_dma_start_transfer) for drv_dma_start_transfer
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_set_int) for drv_wdg_set_int
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_clear_counter) for drv_wdg_clear_counter
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_read_edge_flag) for drv_wdg_read_edge_flag
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_clear_edge_flag) for drv_wdg_clear_edge_flag
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(.data) for .data
    drv_wdg.o(i.drv_wdg_register_callback) refers to drv_wdg.o(.data) for .data
    drv_wdg.o(i.drv_wdg_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_wdg.o(i.drv_wdg_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_wdg.o(i.drv_wdg_set_repeat) refers to drv_wdg.o(.data) for .data
    dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_fifo_init) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_size) refers to dcs_packet_fifo.o(.bss) for .bss
    ceil.o(i.__softfp_ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.__softfp_ceil) refers to ceil.o(i.ceil) for ceil
    ceil.o(i.ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.ceil) refers to dadd.o(.text) for __aeabi_dadd
    ceil.o(i.ceil) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    sqrt.o(i.__softfp_sqrt) refers (Special) to iusefp.o(.text) for __I$use$fp
    sqrt.o(i.__softfp_sqrt) refers to dsqrt.o(.text) for _dsqrt
    sqrt.o(i.__softfp_sqrt) refers to errno.o(i.__set_errno) for __set_errno
    sqrt.o(i.sqrt) refers (Special) to iusefp.o(.text) for __I$use$fp
    sqrt.o(i.sqrt) refers to dsqrt.o(.text) for _dsqrt
    sqrt.o(i.sqrt) refers to errno.o(i.__set_errno) for __set_errno
    sqrt_x.o(i.____softfp_sqrt$lsc) refers (Special) to iusefp.o(.text) for __I$use$fp
    sqrt_x.o(i.____softfp_sqrt$lsc) refers to cdcmple.o(.text) for __aeabi_cdcmple
    sqrt_x.o(i.____softfp_sqrt$lsc) refers to errno.o(i.__set_errno) for __set_errno
    sqrt_x.o(i.____softfp_sqrt$lsc) refers to dsqrt.o(.text) for _dsqrt
    sqrt_x.o(i.__sqrt$lsc) refers (Special) to iusefp.o(.text) for __I$use$fp
    sqrt_x.o(i.__sqrt$lsc) refers to cdcmple.o(.text) for __aeabi_cdcmple
    sqrt_x.o(i.__sqrt$lsc) refers to errno.o(i.__set_errno) for __set_errno
    sqrt_x.o(i.__sqrt$lsc) refers to dsqrt.o(.text) for _dsqrt
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry10a.o(.ARM.Collect$$$$0000000D) for __rt_final_cpp
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry11a.o(.ARM.Collect$$$$0000000F) for __rt_final_exit
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry7b.o(.ARM.Collect$$$$00000008) for _main_clock
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry8b.o(.ARM.Collect$$$$0000000A) for _main_cpp_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry9a.o(.ARM.Collect$$$$0000000B) for _main_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry5.o(.ARM.Collect$$$$00000004) for _main_scatterload
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry2.o(.ARM.Collect$$$$00000001) for _main_stk
    idiv.o(.text) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfb.o(i.__0fprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0fprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0printf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printfb.o(i.__0vfprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vfprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printf0.o(i.__0fprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0fprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0printf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf0.o(i.__0vfprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vfprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf1.o(i.__0fprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0fprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0printf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i.__0vfprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vfprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf2.o(i.__0fprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0fprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0printf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf2.o(i.__0vfprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vfprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf3.o(i.__0fprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0fprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0printf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i.__0vfprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vfprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf4.o(i.__0fprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0fprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0printf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i.__0vfprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vfprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf5.o(i.__0fprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0fprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0printf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i.__0vfprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vfprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf6.o(i.__0fprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0fprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0printf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i.__0vfprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vfprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i._printf_core) refers to printf6.o(i._printf_pre_padding) for _printf_pre_padding
    printf6.o(i._printf_core) refers to printf6.o(i._printf_post_padding) for _printf_post_padding
    printf6.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf7.o(i.__0fprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0fprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0printf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i.__0vfprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vfprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i._printf_core) refers to printf7.o(i._printf_pre_padding) for _printf_pre_padding
    printf7.o(i._printf_core) refers to printf7.o(i._printf_post_padding) for _printf_post_padding
    printf7.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf8.o(i.__0fprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0fprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0printf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i.__0vfprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vfprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i._printf_core) refers to printf8.o(i._printf_pre_padding) for _printf_pre_padding
    printf8.o(i._printf_core) refers to printf8.o(i._printf_post_padding) for _printf_post_padding
    printf8.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i.__0fprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0fprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0fprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0printf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0printf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0snprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0snprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0snprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0sprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0sprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0sprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i.__0vfprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vfprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vfprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0vsnprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0vsprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i._fp_digits) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._fp_digits) refers to dmul.o(.text) for __aeabi_dmul
    printfa.o(i._fp_digits) refers to ddiv.o(.text) for __aeabi_ddiv
    printfa.o(i._fp_digits) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    printfa.o(i._fp_digits) refers to dadd.o(.text) for __aeabi_dadd
    printfa.o(i._fp_digits) refers to dfixul.o(.text) for __aeabi_d2ulz
    printfa.o(i._fp_digits) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_core) refers to printfa.o(i._printf_pre_padding) for _printf_pre_padding
    printfa.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers to printfa.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i._printf_core) refers to printfa.o(i._fp_digits) for _fp_digits
    printfa.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfa.o(i._printf_post_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_pre_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._snputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._sputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    fmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers to fepilogue.o(.text) for _float_round
    fscalb.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    dadd.o(.text) refers to llsshr.o(.text) for __aeabi_lasr
    dadd.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dmul.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ddiv.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ddiv.o(.text) refers to depilogue.o(.text) for _double_round
    fflti.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fflti.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    ffltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ffltui.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    dflti.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dflti.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dfltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfltui.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ffixi.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ffixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixi.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixi.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixui.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    f2d.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    cdcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    cfcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    cfrcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    entry2.o(.ARM.Collect$$$$00000001) refers to entry2.o(.ARM.Collect$$$$00002712) for __lit__00000000
    entry2.o(.ARM.Collect$$$$00002712) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    entry5.o(.ARM.Collect$$$$00000004) refers to init.o(.text) for __scatterload
    entry9a.o(.ARM.Collect$$$$0000000B) refers to main.o(i.main) for main
    entry9b.o(.ARM.Collect$$$$0000000C) refers to main.o(i.main) for main
    uldiv.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    uldiv.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    errno.o(i.__aeabi_errno_addr) refers to errno.o(.data) for .data
    errno.o(i.__read_errno) refers to errno.o(.data) for .data
    errno.o(i.__set_errno) refers to errno.o(.data) for .data
    depilogue.o(.text) refers to depilogue.o(i.__ARM_clz) for __ARM_clz
    depilogue.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dsqrt.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dsqrt.o(.text) refers to depilogue.o(.text) for _double_round
    dfixul.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixul.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    init.o(.text) refers to entry5.o(.ARM.Collect$$$$00000004) for __main_after_scatterload


==============================================================================

Removing Unused input sections from the image.

    Removing main.o(.rev16_text), (4 bytes).
    Removing main.o(.revsh_text), (4 bytes).
    Removing ap_demo.o(.rev16_text), (4 bytes).
    Removing ap_demo.o(.revsh_text), (4 bytes).
    Removing ap_demo.o(i.ap_get_finger_flag), (136 bytes).
    Removing ap_demo.o(i.ap_get_reg_ca), (28 bytes).
    Removing ap_demo.o(i.ap_get_reg_df), (368 bytes).
    Removing ap_demo.o(i.ap_reset_high), (16 bytes).
    Removing ap_demo.o(i.ap_reset_low), (88 bytes).
    Removing ap_demo.o(i.ap_set_backlight), (684 bytes).
    Removing ap_demo.o(i.finger_calibration_time_counter_exec), (56 bytes).
    Removing ap_demo.o(i.soft_swire_init), (52 bytes).
    Removing ap_demo.o(i.soft_swire_start), (46 bytes).
    Removing ap_demo.o(i.soft_swire_timer_callback), (36 bytes).
    Removing ap_demo.o(i.swire_callback), (24 bytes).
    Removing ap_demo.o(i.swire_init), (68 bytes).
    Removing ap_demo.o(i.swire_timer_callback), (28 bytes).
    Removing app_tp_transfer.o(.rev16_text), (4 bytes).
    Removing app_tp_transfer.o(.revsh_text), (4 bytes).
    Removing app_tp_transfer.o(i.ap_doubleclick), (32 bytes).
    Removing app_tp_transfer.o(i.ap_doubleclick_1), (32 bytes).
    Removing app_tp_transfer.o(i.app_tp_phone_reset_on), (12 bytes).
    Removing app_tp_transfer.o(i.app_tp_s_transfer_complate), (26 bytes).
    Removing app_tp_st_touch.o(.rev16_text), (4 bytes).
    Removing app_tp_st_touch.o(.revsh_text), (4 bytes).
    Removing app_tp_st_touch.o(i.ap_tp_st_touch_software_reset), (124 bytes).
    Removing board.o(.rev16_text), (4 bytes).
    Removing board.o(.revsh_text), (4 bytes).
    Removing startup_armcm0.o(HEAP), (3072 bytes).
    Removing hal_dsi_rx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_short_cmd), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video), (228 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init), (48 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern), (216 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en), (16 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode), (100 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_write_cmd_entry), (10 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle), (40 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart), (80 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk), (44 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line), (52 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_dcs_direct_mode), (8 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter), (40 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format), (56 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data), (148 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data), (268 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk), (80 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_te_waveform), (52 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate), (10 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution_ex), (32 bytes).
    Removing hal_dsi_tx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic), (148 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode_rcv_te), (10 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard), (280 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker), (172 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_mode_init), (30 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_ulps_mode), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_ulps_mode), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd), (140 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle), (28 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_pq_filter), (28 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_lp_cmd), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data), (272 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg), (80 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd), (240 bytes).
    Removing hal_gpio.o(.rev16_text), (4 bytes).
    Removing hal_gpio.o(.revsh_text), (4 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_int_type), (20 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_pull_state), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_driving_strength), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_output_data_ex), (36 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_schmitt_trigger), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_slew_rate), (32 bytes).
    Removing hal_i2c_master.o(.rev16_text), (4 bytes).
    Removing hal_i2c_master.o(.revsh_text), (4 bytes).
    Removing hal_i2c_master.o(i.hal_i2c_m_deinit), (8 bytes).
    Removing hal_i2c_master.o(i.hal_i2c_m_set_high_impedance), (46 bytes).
    Removing hal_i2c_slave.o(.rev16_text), (4 bytes).
    Removing hal_i2c_slave.o(.revsh_text), (4 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_deinit), (88 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_get_tx_byte_num), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_read_complate), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_read_complate_clear), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_read_data), (32 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_rxfifo_notempty), (40 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_sel), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_set_dma_tx_cycle), (36 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance), (88 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_write_complate), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_write_data), (32 bytes).
    Removing hal_spi_master.o(.rev16_text), (4 bytes).
    Removing hal_spi_master.o(.revsh_text), (4 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_callback), (24 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_deinit), (10 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_dma_init), (104 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_dma_read), (36 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_dma_write), (40 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_get_transfer_complate), (36 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_gpio_init), (8 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_read_rxfifo), (28 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_set_high_impedance), (100 bytes).
    Removing hal_spi_master.o(.data), (1 bytes).
    Removing hal_swire.o(.rev16_text), (4 bytes).
    Removing hal_swire.o(.revsh_text), (4 bytes).
    Removing hal_swire.o(i.hal_swire_init), (32 bytes).
    Removing hal_swire.o(i.hal_swire_register_callback), (10 bytes).
    Removing hal_swire.o(i.hal_swire_start), (108 bytes).
    Removing hal_system.o(.rev16_text), (4 bytes).
    Removing hal_system.o(.revsh_text), (4 bytes).
    Removing hal_system.o(i.hal_system_clear_debug_state), (10 bytes).
    Removing hal_system.o(i.hal_system_deep_sleep_mode), (8 bytes).
    Removing hal_system.o(i.hal_system_disable_systick), (8 bytes).
    Removing hal_system.o(i.hal_system_get_debug_state), (8 bytes).
    Removing hal_system.o(i.hal_system_get_tick), (8 bytes).
    Removing hal_system.o(i.hal_system_idle_mode), (8 bytes).
    Removing hal_system.o(i.hal_system_register_systick_cb), (8 bytes).
    Removing hal_system.o(i.hal_system_reset_chip), (32 bytes).
    Removing hal_system.o(i.hal_system_share_flash_mode), (20 bytes).
    Removing hal_system.o(i.hal_system_sleep_mode), (48 bytes).
    Removing hal_timer.o(.rev16_text), (4 bytes).
    Removing hal_timer.o(.revsh_text), (4 bytes).
    Removing hal_timer.o(i.hal_timer_get_status), (8 bytes).
    Removing hal_timer.o(i.hal_timer_set_repeat), (8 bytes).
    Removing hal_timer.o(i.hal_timer_start_ex), (72 bytes).
    Removing tau_delay.o(.rev16_text), (4 bytes).
    Removing tau_delay.o(.revsh_text), (4 bytes).
    Removing tau_log.o(.rev16_text), (4 bytes).
    Removing tau_log.o(.revsh_text), (4 bytes).
    Removing tau_log.o(i.fgetc), (22 bytes).
    Removing app_tp_for_custom_s8.o(.rev16_text), (4 bytes).
    Removing app_tp_for_custom_s8.o(.revsh_text), (4 bytes).
    Removing app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const), (180 bytes).
    Removing hal_uart.o(.rev16_text), (4 bytes).
    Removing hal_uart.o(.revsh_text), (4 bytes).
    Removing hal_uart.o(i.hal_uart_deinit), (28 bytes).
    Removing hal_uart.o(i.hal_uart_dmacallback), (36 bytes).
    Removing hal_uart.o(i.hal_uart_receive_blocking), (16 bytes).
    Removing hal_uart.o(i.hal_uart_receive_dma), (76 bytes).
    Removing hal_uart.o(i.hal_uart_transmit_dma), (76 bytes).
    Removing hal_internal_vsync.o(.rev16_text), (4 bytes).
    Removing hal_internal_vsync.o(.revsh_text), (4 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te), (168 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex), (468 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual), (512 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_register_write_cmd_entry), (12 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode), (48 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line), (68 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate), (152 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_update_lcdc_addr), (48 bytes).
    Removing hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler), (476 bytes).
    Removing drv_common.o(.rev16_text), (4 bytes).
    Removing drv_common.o(.revsh_text), (4 bytes).
    Removing drv_common.o(i.drv_common_disable_systick), (20 bytes).
    Removing drv_common.o(i.drv_common_get_tick), (12 bytes).
    Removing drv_common.o(i.drv_common_idle_mode), (40 bytes).
    Removing drv_common.o(i.drv_common_systick_register_cb), (12 bytes).
    Removing drv_crgu.o(.rev16_text), (4 bytes).
    Removing drv_crgu.o(.revsh_text), (4 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_all_reset_flags), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_reset_flag), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_config_clocks), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_config_clocks_div), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_config_clocks_src), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_ana_clk_status), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_clocks), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_fpga_id), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_mipi_ref_src), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_reset_flag), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_system_clk), (28 bytes).
    Removing drv_crgu.o(i.drv_crgu_reset_chip), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_200m_scan_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_300m_scan_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_abp0_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_adc_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_adc_src), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_apb1_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_apb2_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_fls_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_fls_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_monitor_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_monitor_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_swire_div), (20 bytes).
    Removing drv_dma.o(.rev16_text), (4 bytes).
    Removing drv_dma.o(.revsh_text), (4 bytes).
    Removing drv_dma.o(i.drv_dma_abort_transfer), (32 bytes).
    Removing drv_dma.o(i.drv_dma_ahb_init), (74 bytes).
    Removing drv_dma.o(i.drv_dma_channel_is_active), (20 bytes).
    Removing drv_dma.o(i.drv_dma_deinit), (32 bytes).
    Removing drv_dma.o(i.drv_dma_disenable_channel_interrupts), (24 bytes).
    Removing drv_dma.o(i.drv_dma_enable_cycle), (44 bytes).
    Removing drv_dma.o(i.drv_dma_get_remaining_bytes), (32 bytes).
    Removing drv_dma.o(i.drv_dma_init), (24 bytes).
    Removing drv_dma.o(i.drv_dma_m2m_init), (72 bytes).
    Removing drv_dma.o(i.drv_dma_reset), (10 bytes).
    Removing drv_dma.o(i.drv_dma_set_ccr), (114 bytes).
    Removing drv_dma.o(i.drv_dma_start_transfer), (32 bytes).
    Removing drv_fls.o(.rev16_text), (4 bytes).
    Removing drv_fls.o(.revsh_text), (4 bytes).
    Removing drv_fls.o(i.__NVIC_DisableIRQ), (32 bytes).
    Removing drv_fls.o(i.drv_fls_gpio_connect), (28 bytes).
    Removing drv_fls.o(i.drv_fls_gpio_disconnect), (32 bytes).
    Removing drv_fls.o(i.fls_EnableClk), (12 bytes).
    Removing drv_fls.o(i.fls_busy_pending), (12 bytes).
    Removing drv_fls.o(i.fls_clear_irq_status), (6 bytes).
    Removing drv_fls.o(i.fls_ctrl_cfg_init), (72 bytes).
    Removing drv_fls.o(i.fls_ddat_enable), (24 bytes).
    Removing drv_fls.o(i.fls_de_init), (52 bytes).
    Removing drv_fls.o(i.fls_descr), (10 bytes).
    Removing drv_fls.o(i.fls_disable_it), (36 bytes).
    Removing drv_fls.o(i.fls_en_scr), (10 bytes).
    Removing drv_fls.o(i.fls_enable_it), (48 bytes).
    Removing drv_fls.o(i.fls_get_crcout), (4 bytes).
    Removing drv_fls.o(i.fls_get_default_fls_config), (20 bytes).
    Removing drv_fls.o(i.fls_get_default_spi_config), (44 bytes).
    Removing drv_fls.o(i.fls_get_default_tuning), (12 bytes).
    Removing drv_fls.o(i.fls_get_tuning), (18 bytes).
    Removing drv_fls.o(i.fls_init), (62 bytes).
    Removing drv_fls.o(i.fls_qadr_enable), (22 bytes).
    Removing drv_fls.o(i.fls_qcmd_enable), (22 bytes).
    Removing drv_fls.o(i.fls_qdat_enable), (22 bytes).
    Removing drv_fls.o(i.fls_read_byte_data), (130 bytes).
    Removing drv_fls.o(i.fls_read_cmd), (104 bytes).
    Removing drv_fls.o(i.fls_read_cmd_it), (110 bytes).
    Removing drv_fls.o(i.fls_reset_crc), (18 bytes).
    Removing drv_fls.o(i.fls_scr_clear), (10 bytes).
    Removing drv_fls.o(i.fls_set_addr_dummy), (32 bytes).
    Removing drv_fls.o(i.fls_set_addr_len), (32 bytes).
    Removing drv_fls.o(i.fls_set_mc_irq_mask), (26 bytes).
    Removing drv_fls.o(i.fls_set_read), (10 bytes).
    Removing drv_fls.o(i.fls_set_tuning), (24 bytes).
    Removing drv_fls.o(i.fls_set_write), (10 bytes).
    Removing drv_fls.o(i.fls_single_mode), (16 bytes).
    Removing drv_fls.o(i.fls_spi_init), (180 bytes).
    Removing drv_fls.o(i.fls_spi_start), (10 bytes).
    Removing drv_fls.o(i.fls_swrst), (18 bytes).
    Removing drv_fls.o(i.fls_write_byte_data), (164 bytes).
    Removing drv_fls.o(i.fls_write_cmd), (58 bytes).
    Removing drv_fls.o(.data), (4 bytes).
    Removing drv_gpio.o(.rev16_text), (4 bytes).
    Removing drv_gpio.o(.revsh_text), (4 bytes).
    Removing drv_gpio.o(i.drv_gpio_get_pull_state), (224 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_driving_strength), (312 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_schmitt_trigger), (168 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_slew_rate), (168 bytes).
    Removing drv_i2c_dma.o(.rev16_text), (4 bytes).
    Removing drv_i2c_dma.o(.revsh_text), (4 bytes).
    Removing drv_i2c_master.o(.rev16_text), (4 bytes).
    Removing drv_i2c_master.o(.revsh_text), (4 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_bus_init), (36 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_deinit), (80 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_disable_intr), (16 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_get_fifo_status), (28 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_read_data), (32 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_set_fifo_threshold), (24 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_set_sys_mask), (48 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_write_data), (32 bytes).
    Removing drv_i2c_slave.o(.rev16_text), (4 bytes).
    Removing drv_i2c_slave.o(.revsh_text), (4 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_read_data), (30 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_set_fifo_threshold), (16 bytes).
    Removing drv_param_init.o(.rev16_text), (4 bytes).
    Removing drv_param_init.o(.revsh_text), (4 bytes).
    Removing drv_param_init.o(i.drv_param_init_set_sclu_filter), (28 bytes).
    Removing drv_pwr.o(.rev16_text), (4 bytes).
    Removing drv_pwr.o(.revsh_text), (4 bytes).
    Removing drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_frame_buff_pd), (28 bytes).
    Removing drv_spi_dma.o(.rev16_text), (4 bytes).
    Removing drv_spi_dma.o(.revsh_text), (4 bytes).
    Removing drv_spi_dma.o(i.__NVIC_ClearPendingIRQ), (24 bytes).
    Removing drv_spi_dma.o(i.drv_spi_abort_dma), (108 bytes).
    Removing drv_spi_dma.o(i.drv_spi_dma_callback), (60 bytes).
    Removing drv_spi_dma.o(i.drv_spi_dma_ch6_init), (208 bytes).
    Removing drv_spi_dma.o(i.drv_spi_dma_init), (220 bytes).
    Removing drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback), (48 bytes).
    Removing drv_spi_dma.o(i.drv_spi_set_dma_irq_callback), (88 bytes).
    Removing drv_spi_dma.o(i.drv_spim_dma_read), (96 bytes).
    Removing drv_spi_dma.o(i.drv_spim_dma_write), (60 bytes).
    Removing drv_spi_dma.o(i.drv_spis_dma_write), (72 bytes).
    Removing drv_spi_dma.o(.bss), (480 bytes).
    Removing drv_spi_dma.o(.data), (16 bytes).
    Removing drv_spi_master.o(.rev16_text), (4 bytes).
    Removing drv_spi_master.o(.revsh_text), (4 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_deinit), (40 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_disable_int), (68 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_enable_int), (72 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_enable_rx_dma), (32 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_enable_tx_dma), (28 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_get_dma_address), (8 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_gpio_init), (32 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_set_intr_callback), (12 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_switch_sclk), (28 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_write_data), (44 bytes).
    Removing drv_spi_master.o(i.drv_spi_master_init), (164 bytes).
    Removing drv_swire.o(.rev16_text), (4 bytes).
    Removing drv_swire.o(.revsh_text), (4 bytes).
    Removing drv_swire.o(i.drv_swire_register_callback), (12 bytes).
    Removing drv_swire.o(i.drv_swire_set_bit_time), (24 bytes).
    Removing drv_swire.o(i.drv_swire_set_pulse_count), (12 bytes).
    Removing drv_sys_cfg.o(.rev16_text), (4 bytes).
    Removing drv_sys_cfg.o(.revsh_text), (4 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_dma_req_mask), (32 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_read_version0_id), (12 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_set_ap_reset), (28 bytes).
    Removing drv_timer.o(.rev16_text), (4 bytes).
    Removing drv_timer.o(.revsh_text), (4 bytes).
    Removing drv_timer.o(i.drv_timer_get_status), (38 bytes).
    Removing hal_internal_soft_sync.o(.rev16_text), (4 bytes).
    Removing hal_internal_soft_sync.o(.revsh_text), (4 bytes).
    Removing hal_internal_soft_sync.o(i.hal_intl_svs_deinit_rx), (48 bytes).
    Removing hal_internal_soft_sync.o(i.hal_intl_svs_set_input_frate), (120 bytes).
    Removing hal_internal_soft_sync.o(i.hal_intl_svs_set_sync_coef), (12 bytes).
    Removing drv_dsi_rx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_rx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate), (66 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_version), (4 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration), (236 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg), (32 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg), (48 bytes).
    Removing drv_dsi_rx.o(i.drv_rx_phy_test_read), (12 bytes).
    Removing drv_dsi_tx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_tx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_force_interrupt), (8 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_get_phy_status), (6 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_forcepll), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration), (232 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_start), (18 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock), (10 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot), (62 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger), (92 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter), (344 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit), (276 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_sdf_3d), (28 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_bta), (22 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_vpg), (70 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_version), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_vid_shadow), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_read), (10 bytes).
    Removing drv_lcdc.o(.rev16_text), (4 bytes).
    Removing drv_lcdc.o(.revsh_text), (4 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_config_rgb_to_pentile), (6 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_enable), (42 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_update_shadow_reg), (12 bytes).
    Removing drv_memc.o(.rev16_text), (4 bytes).
    Removing drv_memc.o(.revsh_text), (4 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_frm_time), (14 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_int_frame), (28 bytes).
    Removing drv_memc.o(i.drv_memc_set_fb_remaining_line_trigger), (12 bytes).
    Removing drv_memc.o(i.drv_memc_set_read_trigger_line), (16 bytes).
    Removing drv_memc.o(i.drv_memc_set_te_ind), (16 bytes).
    Removing drv_memc.o(i.drv_memc_set_tear_hwclr), (16 bytes).
    Removing drv_memc.o(i.drv_memc_set_vidc_fb_arb), (14 bytes).
    Removing drv_memc.o(i.drv_memc_set_write_trigger_line), (16 bytes).
    Removing drv_rxbr.o(.rev16_text), (4 bytes).
    Removing drv_rxbr.o(.revsh_text), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_dsc_flush), (16 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_cur_hline_rcv_cnt), (8 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_ipi_vsync_interval), (8 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_pix_fmt), (8 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_cmd_filter), (204 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_col_addr), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_compress), (24 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_page_addr), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_soft_reset), (98 bytes).
    Removing drv_vidc.o(.rev16_text), (4 bytes).
    Removing drv_vidc.o(.revsh_text), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_clear_status0), (14 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_cap_pixel), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_signal_frame), (30 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_int_source), (38 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status0), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status1), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status2), (6 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_dsc_thresh), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_frmst_latency), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_inff_thresh), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_irq_line), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_module_enable), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_outff_thresh), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_update_src_format), (14 bytes).
    Removing irq_redirect .o(.rev16_text), (4 bytes).
    Removing irq_redirect .o(.revsh_text), (4 bytes).
    Removing drv_efuse.o(.rev16_text), (4 bytes).
    Removing drv_efuse.o(.revsh_text), (4 bytes).
    Removing drv_efuse.o(i.drv_efuse_crc_cal), (128 bytes).
    Removing drv_efuse.o(i.drv_efuse_get_default_config), (26 bytes).
    Removing drv_efuse.o(i.drv_efuse_int_disable), (12 bytes).
    Removing drv_efuse.o(i.drv_efuse_write), (46 bytes).
    Removing drv_efuse.o(i.drv_efuse_write_req), (22 bytes).
    Removing drv_phy_common.o(.rev16_text), (4 bytes).
    Removing drv_phy_common.o(.revsh_text), (4 bytes).
    Removing drv_phy_common.o(i.drv_phy_test_read), (8 bytes).
    Removing drv_chip_info.o(.rev16_text), (4 bytes).
    Removing drv_chip_info.o(.revsh_text), (4 bytes).
    Removing drv_dsc_dec.o(.rev16_text), (4 bytes).
    Removing drv_dsc_dec.o(.revsh_text), (4 bytes).
    Removing drv_dsc_dec.o(i.drv_dsc_dec_set_u32_pps), (120 bytes).
    Removing hal_spi_slave.o(.rev16_text), (4 bytes).
    Removing hal_spi_slave.o(.revsh_text), (4 bytes).
    Removing hal_spi_slave.o(i.hal_spi_s_set_high_impedance), (100 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_auto_transfer_abort), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start), (56 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_busy), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_deinit), (10 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_disable), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_enable), (96 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_flush_fifo), (20 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_get_rxfifo_notempty), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_gpio_init), (8 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_init), (76 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_read_data), (10 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_register_callback), (12 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_reset_tx), (68 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_set_auto_rx_buffer), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_set_auto_tx_buffer), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_write_data), (14 bytes).
    Removing norflash.o(.rev16_text), (4 bytes).
    Removing norflash.o(.revsh_text), (4 bytes).
    Removing norflash.o(i.norflash_best_cfg_init), (44 bytes).
    Removing norflash.o(i.norflash_big_end_clear), (14 bytes).
    Removing norflash.o(i.norflash_big_end_enable), (20 bytes).
    Removing norflash.o(i.norflash_check_crc32), (14 bytes).
    Removing norflash.o(i.norflash_check_id), (72 bytes).
    Removing norflash.o(i.norflash_dma_callback), (24 bytes).
    Removing norflash.o(i.norflash_dma_read), (156 bytes).
    Removing norflash.o(i.norflash_dma_write), (252 bytes).
    Removing norflash.o(i.norflash_dual_read), (60 bytes).
    Removing norflash.o(i.norflash_dual_write), (112 bytes).
    Removing norflash.o(i.norflash_en4b), (40 bytes).
    Removing norflash.o(i.norflash_en_quad), (116 bytes).
    Removing norflash.o(i.norflash_en_quad_check), (64 bytes).
    Removing norflash.o(i.norflash_erase_block), (44 bytes).
    Removing norflash.o(i.norflash_erase_chip), (28 bytes).
    Removing norflash.o(i.norflash_erase_sector), (44 bytes).
    Removing norflash.o(i.norflash_ex4b), (40 bytes).
    Removing norflash.o(i.norflash_exit_quad), (76 bytes).
    Removing norflash.o(i.norflash_get_dual_hstatus), (52 bytes).
    Removing norflash.o(i.norflash_get_hstatus), (52 bytes).
    Removing norflash.o(i.norflash_get_status), (52 bytes).
    Removing norflash.o(i.norflash_init), (48 bytes).
    Removing norflash.o(i.norflash_quad_read), (76 bytes).
    Removing norflash.o(i.norflash_quad_write), (108 bytes).
    Removing norflash.o(i.norflash_read), (28 bytes).
    Removing norflash.o(i.norflash_read_config_reg), (36 bytes).
    Removing norflash.o(i.norflash_read_id), (20 bytes).
    Removing norflash.o(i.norflash_read_uid), (52 bytes).
    Removing norflash.o(i.norflash_reset), (2 bytes).
    Removing norflash.o(i.norflash_reset_crc32), (32 bytes).
    Removing norflash.o(i.norflash_set_best_cfg), (50 bytes).
    Removing norflash.o(i.norflash_set_best_read_cfg), (84 bytes).
    Removing norflash.o(i.norflash_set_best_write_cfg), (84 bytes).
    Removing norflash.o(i.norflash_switch_fls_spi), (112 bytes).
    Removing norflash.o(i.norflash_write), (96 bytes).
    Removing norflash.o(i.norflash_write_disable), (64 bytes).
    Removing norflash.o(i.norflash_write_enable), (56 bytes).
    Removing norflash.o(i.norflash_write_endian_scr), (132 bytes).
    Removing norflash.o(.bss), (412 bytes).
    Removing norflash.o(.bss), (32 bytes).
    Removing norflash.o(.data), (2 bytes).
    Removing drv_fls_dma.o(.rev16_text), (4 bytes).
    Removing drv_fls_dma.o(.revsh_text), (4 bytes).
    Removing drv_fls_dma.o(i.fls_abort_dma), (42 bytes).
    Removing drv_fls_dma.o(i.fls_dma_disable), (10 bytes).
    Removing drv_fls_dma.o(i.fls_dma_enable), (10 bytes).
    Removing drv_fls_dma.o(i.fls_dma_read_prepare), (86 bytes).
    Removing drv_fls_dma.o(i.fls_dma_write_prepare), (82 bytes).
    Removing drv_fls_dma.o(i.fls_read_dmacallback), (32 bytes).
    Removing drv_fls_dma.o(i.fls_transfer_create_handle_dma), (208 bytes).
    Removing drv_fls_dma.o(i.fls_transfer_dma), (112 bytes).
    Removing drv_fls_dma.o(i.fls_transfer_get_receive_count_dma), (44 bytes).
    Removing drv_fls_dma.o(i.fls_write_dmacallback), (32 bytes).
    Removing drv_fls_dma.o(.data), (8 bytes).
    Removing drv_pwm.o(.rev16_text), (4 bytes).
    Removing drv_pwm.o(.revsh_text), (4 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_clear_pwm_int_all), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_enable), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_counter_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_current_count), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_high_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_low_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_register_callback), (24 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_set_pwm_int), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_set_sys_int), (64 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_enable), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_get_sync_flag), (16 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_pause), (28 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_control), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_sync_mode), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_threshold), (12 bytes).
    Removing drv_spi_slave.o(.rev16_text), (4 bytes).
    Removing drv_spi_slave.o(.revsh_text), (4 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_deinit), (40 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_disable_int), (68 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_enable_int), (72 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_enable_rx_dma), (32 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_enable_tx_dma), (28 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_get_dma_address), (8 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_gpio_init), (24 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_read_data), (32 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_switch_sclk), (28 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_write_data), (44 bytes).
    Removing drv_spi_slave.o(i.drv_spi_slave_init), (76 bytes).
    Removing drv_uart.o(.rev16_text), (4 bytes).
    Removing drv_uart.o(.revsh_text), (4 bytes).
    Removing drv_uart.o(i.UART_AbortReceive), (30 bytes).
    Removing drv_uart.o(i.UART_AbortSend), (30 bytes).
    Removing drv_uart.o(i.UART_Deinit), (28 bytes).
    Removing drv_uart.o(i.UART_Disable_IT), (68 bytes).
    Removing drv_uart.o(i.UART_EnableDma), (32 bytes).
    Removing drv_uart.o(i.UART_Enable_IT), (44 bytes).
    Removing drv_uart.o(i.UART_GetDefaultConfig), (72 bytes).
    Removing drv_uart.o(i.UART_GetFIFO_Ctrl), (20 bytes).
    Removing drv_uart.o(i.UART_GetReceiveCount), (22 bytes).
    Removing drv_uart.o(i.UART_GetReceiveStatus), (20 bytes).
    Removing drv_uart.o(i.UART_GetRxRingBufferLength), (28 bytes).
    Removing drv_uart.o(i.UART_GetSendCount), (22 bytes).
    Removing drv_uart.o(i.UART_GetSendStatus), (20 bytes).
    Removing drv_uart.o(i.UART_ReadBlocking), (32 bytes).
    Removing drv_uart.o(i.UART_ReceiveNonBlocking), (50 bytes).
    Removing drv_uart.o(i.UART_ResetTxFIFO), (36 bytes).
    Removing drv_uart.o(i.UART_SendNonBlocking), (38 bytes).
    Removing drv_uart.o(i.UART_TransferCreateHandle), (96 bytes).
    Removing drv_uart.o(i.UART_TransferStartRingBuffer), (30 bytes).
    Removing drv_uart.o(.constdata), (1 bytes).
    Removing drv_uart_dma.o(.rev16_text), (4 bytes).
    Removing drv_uart_dma.o(.revsh_text), (4 bytes).
    Removing drv_uart_dma.o(i.UART_DMAInit), (76 bytes).
    Removing drv_uart_dma.o(i.UART_TransferAbortReceiveDMA), (16 bytes).
    Removing drv_uart_dma.o(i.UART_TransferAbortSendDMA), (16 bytes).
    Removing drv_uart_dma.o(i.UART_TransferCreateHandleDMA), (176 bytes).
    Removing drv_uart_dma.o(i.UART_TransferGetReceiveCountDMA), (44 bytes).
    Removing drv_uart_dma.o(i.UART_TransferReceiveDMA), (68 bytes).
    Removing drv_uart_dma.o(i.UART_TransferReceiveDMACallback), (34 bytes).
    Removing drv_uart_dma.o(i.UART_TransferSendDMA), (68 bytes).
    Removing drv_uart_dma.o(i.UART_TransferSendDMACallback), (34 bytes).
    Removing drv_uart_dma.o(.data), (8 bytes).
    Removing drv_wdg.o(.rev16_text), (4 bytes).
    Removing drv_wdg.o(.revsh_text), (4 bytes).
    Removing drv_wdg.o(i.drv_wdg_enable), (32 bytes).
    Removing drv_wdg.o(i.drv_wdg_load_match), (12 bytes).
    Removing drv_wdg.o(i.drv_wdg_register_callback), (12 bytes).
    Removing drv_wdg.o(i.drv_wdg_sel_mode), (28 bytes).
    Removing drv_wdg.o(i.drv_wdg_set_repeat), (12 bytes).
    Removing dcs_packet_fifo.o(i.dcs_packet_get_fifo_size), (16 bytes).
    Removing dflti.o(.text), (40 bytes).

554 unused section(s) (total 27648 bytes) removed from the image.

==============================================================================

Image Symbol Table

    Local Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    ../clib/../cmprslib/zerorunl2.c          0x00000000   Number         0  __dczerorl2.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uldiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  idiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uidiv.o ABSOLUTE
    ../clib/microlib/errno.c                 0x00000000   Number         0  errno.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry5.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry2.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llushr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llsshr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llshl.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfa.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf8.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf7.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf6.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf5.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf4.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf3.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf2.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf1.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf0.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfb.o ABSOLUTE
    ../clib/microlib/printf/stubs.s          0x00000000   Number         0  stubs.o ABSOLUTE
    ../clib/microlib/stdio/streams.c         0x00000000   Number         0  stdout.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpya.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpyb.o ABSOLUTE
    ../clib/microlib/string/memset.c         0x00000000   Number         0  memseta.o ABSOLUTE
    ../clib/microlib/stubs.s                 0x00000000   Number         0  iusefp.o ABSOLUTE
    ../fplib/microlib/f2d.c                  0x00000000   Number         0  f2d.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  dadd.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  fadd.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  ddiv.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  fdiv.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  depilogue.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  fepilogue.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  ffixi.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  ffixui.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixi.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixui.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixul.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  dfltui.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  dflti.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  ffltui.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  fflti.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  fmul.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  dmul.o ABSOLUTE
    ../fplib/microlib/fpscalb.c              0x00000000   Number         0  fscalb.o ABSOLUTE
    ../fplib/microlib/fpsqrt.c               0x00000000   Number         0  dsqrt.o ABSOLUTE
    ../mathlib/ceil.c                        0x00000000   Number         0  ceil.o ABSOLUTE
    ../mathlib/sqrt.c                        0x00000000   Number         0  sqrt.o ABSOLUTE
    ../mathlib/sqrt.c                        0x00000000   Number         0  sqrt_x.o ABSOLUTE
    ..\..\..\src\common\tau_delay.c          0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\..\..\src\common\tau_log.c            0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\..\..\src\driver\robin\src\drv_chip_info.c 0x00000000   Number         0  drv_chip_info.o ABSOLUTE
    ..\..\..\src\driver\robin\src\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\irq_redirect .c 0x00000000   Number         0  irq_redirect .o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\internal\dcs_packet_fifo.c 0x00000000   Number         0  dcs_packet_fifo.o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\internal\hal_internal_soft_sync.c 0x00000000   Number         0  hal_internal_soft_sync.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_fls.c 0x00000000   Number         0  drv_fls.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_fls_dma.c 0x00000000   Number         0  drv_fls_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_i2c_dma.c 0x00000000   Number         0  drv_i2c_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_i2c_master.c 0x00000000   Number         0  drv_i2c_master.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_i2c_slave.c 0x00000000   Number         0  drv_i2c_slave.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_param_init.c 0x00000000   Number         0  drv_param_init.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_pwm.c 0x00000000   Number         0  drv_pwm.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_spi_dma.c 0x00000000   Number         0  drv_spi_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_spi_master.c 0x00000000   Number         0  drv_spi_master.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_spi_slave.c 0x00000000   Number         0  drv_spi_slave.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_uart_dma.c 0x00000000   Number         0  drv_uart_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_wdg.c 0x00000000   Number         0  drv_wdg.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_i2c_master.c 0x00000000   Number         0  hal_i2c_master.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_i2c_slave.c 0x00000000   Number         0  hal_i2c_slave.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_spi_master.c 0x00000000   Number         0  hal_spi_master.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_spi_slave.c 0x00000000   Number         0  hal_spi_slave.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_swire.c 0x00000000   Number         0  hal_swire.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_timer.c 0x00000000   Number         0  hal_timer.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\internal\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\internal\norflash.c 0x00000000   Number         0  norflash.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_delay.c     0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_log.c       0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\\..\\..\\src\\driver\\robin\\src\\drv_chip_info.c 0x00000000   Number         0  drv_chip_info.o ABSOLUTE
    ..\\..\\..\\src\\driver\\robin\\src\\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\irq_redirect .c 0x00000000   Number         0  irq_redirect .o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\hal\\internal\\hal_internal_soft_sync.c 0x00000000   Number         0  hal_internal_soft_sync.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_fls.c 0x00000000   Number         0  drv_fls.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_fls_dma.c 0x00000000   Number         0  drv_fls_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_i2c_dma.c 0x00000000   Number         0  drv_i2c_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_i2c_master.c 0x00000000   Number         0  drv_i2c_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_i2c_slave.c 0x00000000   Number         0  drv_i2c_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_param_init.c 0x00000000   Number         0  drv_param_init.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_pwm.c 0x00000000   Number         0  drv_pwm.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_spi_dma.c 0x00000000   Number         0  drv_spi_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_spi_master.c 0x00000000   Number         0  drv_spi_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_spi_slave.c 0x00000000   Number         0  drv_spi_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_uart_dma.c 0x00000000   Number         0  drv_uart_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_wdg.c 0x00000000   Number         0  drv_wdg.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_i2c_master.c 0x00000000   Number         0  hal_i2c_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_i2c_slave.c 0x00000000   Number         0  hal_i2c_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_spi_master.c 0x00000000   Number         0  hal_spi_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_spi_slave.c 0x00000000   Number         0  hal_spi_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_swire.c 0x00000000   Number         0  hal_swire.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_timer.c 0x00000000   Number         0  hal_timer.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\internal\\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\internal\\norflash.c 0x00000000   Number         0  norflash.o ABSOLUTE
    ..\\src\\app\\demo\\ap_demo.c            0x00000000   Number         0  ap_demo.o ABSOLUTE
    ..\\src\\app\\demo\\app_tp_for_custom_s8.c 0x00000000   Number         0  app_tp_for_custom_s8.o ABSOLUTE
    ..\\src\\app\\demo\\app_tp_st_touch.c    0x00000000   Number         0  app_tp_st_touch.o ABSOLUTE
    ..\\src\\app\\demo\\app_tp_transfer.c    0x00000000   Number         0  app_tp_transfer.o ABSOLUTE
    ..\\src\\app\\main.c                     0x00000000   Number         0  main.o ABSOLUTE
    ..\\src\\board\\board.c                  0x00000000   Number         0  board.o ABSOLUTE
    ..\src\app\demo\ap_demo.c                0x00000000   Number         0  ap_demo.o ABSOLUTE
    ..\src\app\demo\app_tp_for_custom_s8.c   0x00000000   Number         0  app_tp_for_custom_s8.o ABSOLUTE
    ..\src\app\demo\app_tp_st_touch.c        0x00000000   Number         0  app_tp_st_touch.o ABSOLUTE
    ..\src\app\demo\app_tp_transfer.c        0x00000000   Number         0  app_tp_transfer.o ABSOLUTE
    ..\src\app\main.c                        0x00000000   Number         0  main.o ABSOLUTE
    ..\src\board\board.c                     0x00000000   Number         0  board.o ABSOLUTE
    ..\src\board\startup\startup_ARMCM0.s    0x00000000   Number         0  startup_armcm0.o ABSOLUTE
    cdcmple.s                                0x00000000   Number         0  cdcmple.o ABSOLUTE
    cdrcmple.s                               0x00000000   Number         0  cdrcmple.o ABSOLUTE
    cfcmple.s                                0x00000000   Number         0  cfcmple.o ABSOLUTE
    cfrcmple.s                               0x00000000   Number         0  cfrcmple.o ABSOLUTE
    dc.s                                     0x00000000   Number         0  dc.o ABSOLUTE
    handlers.s                               0x00000000   Number         0  handlers.o ABSOLUTE
    init.s                                   0x00000000   Number         0  init.o ABSOLUTE
    RESET                                    0x00010000   Section      192  startup_armcm0.o(RESET)
    .ARM.Collect$$$$00000000                 0x000100c0   Section        0  entry.o(.ARM.Collect$$$$00000000)
    .ARM.Collect$$$$00000001                 0x000100c0   Section        4  entry2.o(.ARM.Collect$$$$00000001)
    .ARM.Collect$$$$00000004                 0x000100c4   Section        4  entry5.o(.ARM.Collect$$$$00000004)
    .ARM.Collect$$$$00000008                 0x000100c8   Section        0  entry7b.o(.ARM.Collect$$$$00000008)
    .ARM.Collect$$$$0000000A                 0x000100c8   Section        0  entry8b.o(.ARM.Collect$$$$0000000A)
    .ARM.Collect$$$$0000000B                 0x000100c8   Section        8  entry9a.o(.ARM.Collect$$$$0000000B)
    .ARM.Collect$$$$0000000D                 0x000100d0   Section        0  entry10a.o(.ARM.Collect$$$$0000000D)
    .ARM.Collect$$$$0000000F                 0x000100d0   Section        0  entry11a.o(.ARM.Collect$$$$0000000F)
    .ARM.Collect$$$$00002712                 0x000100d0   Section        4  entry2.o(.ARM.Collect$$$$00002712)
    __lit__00000000                          0x000100d0   Data           4  entry2.o(.ARM.Collect$$$$00002712)
    .text                                    0x000100d4   Section      120  startup_armcm0.o(.text)
    .text                                    0x0001014c   Section        0  uidiv.o(.text)
    .text                                    0x00010178   Section        0  idiv.o(.text)
    .text                                    0x000101a0   Section        0  memcpya.o(.text)
    .text                                    0x000101c4   Section        0  memseta.o(.text)
    .text                                    0x000101e8   Section        0  fadd.o(.text)
    .text                                    0x0001029a   Section        0  fmul.o(.text)
    .text                                    0x00010314   Section        0  fdiv.o(.text)
    .text                                    0x00010390   Section        0  fscalb.o(.text)
    .text                                    0x000103a8   Section        0  dadd.o(.text)
    .text                                    0x0001050c   Section        0  dmul.o(.text)
    .text                                    0x000105dc   Section        0  ddiv.o(.text)
    .text                                    0x000106cc   Section        0  fflti.o(.text)
    .text                                    0x000106e2   Section        0  ffltui.o(.text)
    .text                                    0x000106f0   Section        0  dfltui.o(.text)
    .text                                    0x0001070c   Section        0  ffixi.o(.text)
    .text                                    0x0001073e   Section        0  ffixui.o(.text)
    .text                                    0x00010768   Section        0  dfixi.o(.text)
    .text                                    0x000107b0   Section        0  dfixui.o(.text)
    .text                                    0x000107ec   Section        0  f2d.o(.text)
    .text                                    0x00010814   Section       40  cdcmple.o(.text)
    .text                                    0x0001083c   Section       20  cfcmple.o(.text)
    .text                                    0x00010850   Section       20  cfrcmple.o(.text)
    .text                                    0x00010864   Section        0  uldiv.o(.text)
    .text                                    0x000108c4   Section        0  llshl.o(.text)
    .text                                    0x000108e4   Section        0  llushr.o(.text)
    .text                                    0x00010906   Section        0  llsshr.o(.text)
    .text                                    0x0001092c   Section        0  fepilogue.o(.text)
    .text                                    0x0001092c   Section        0  iusefp.o(.text)
    .text                                    0x000109ae   Section        0  depilogue.o(.text)
    .text                                    0x00010a6c   Section        0  dsqrt.o(.text)
    .text                                    0x00010b10   Section        0  dfixul.o(.text)
    .text                                    0x00010b50   Section       40  cdrcmple.o(.text)
    .text                                    0x00010b78   Section       36  init.o(.text)
    .text                                    0x00010b9c   Section        0  __dczerorl2.o(.text)
    i.ADC_IRQn_Handler                       0x00010bf4   Section        0  irq_redirect .o(i.ADC_IRQn_Handler)
    i.AP_NRESET_IRQn_Handler                 0x00010c0c   Section        0  irq_redirect .o(i.AP_NRESET_IRQn_Handler)
    i.CRC16_2                                0x00010c24   Section        0  app_tp_st_touch.o(i.CRC16_2)
    i.DMA_IRQn_Handler                       0x00010c6c   Section        0  irq_redirect .o(i.DMA_IRQn_Handler)
    i.EXTI_INT0_IRQn_Handler                 0x00010c80   Section        0  irq_redirect .o(i.EXTI_INT0_IRQn_Handler)
    i.EXTI_INT1_IRQn_Handler                 0x00010c9c   Section        0  irq_redirect .o(i.EXTI_INT1_IRQn_Handler)
    i.EXTI_INT2_IRQn_Handler                 0x00010cb8   Section        0  irq_redirect .o(i.EXTI_INT2_IRQn_Handler)
    i.EXTI_INT3_IRQn_Handler                 0x00010cd4   Section        0  irq_redirect .o(i.EXTI_INT3_IRQn_Handler)
    i.EXTI_INT4_IRQn_Handler                 0x00010cf0   Section        0  irq_redirect .o(i.EXTI_INT4_IRQn_Handler)
    i.EXTI_INT5_IRQn_Handler                 0x00010d0c   Section        0  irq_redirect .o(i.EXTI_INT5_IRQn_Handler)
    i.EXTI_INT6_IRQn_Handler                 0x00010d28   Section        0  irq_redirect .o(i.EXTI_INT6_IRQn_Handler)
    i.EXTI_INT7_IRQn_Handler                 0x00010d44   Section        0  irq_redirect .o(i.EXTI_INT7_IRQn_Handler)
    i.EncryptCheck                           0x00010d60   Section        0  app_tp_for_custom_s8.o(i.EncryptCheck)
    i.FLSCTRL_IRQn_Handler                   0x00010d80   Section        0  irq_redirect .o(i.FLSCTRL_IRQn_Handler)
    i.Gpio_swire_output                      0x00010d94   Section        0  ap_demo.o(i.Gpio_swire_output)
    i.HardFault_Handler                      0x00010de4   Section        0  irq_redirect .o(i.HardFault_Handler)
    i.I2C0_IRQn_Handler                      0x00010df8   Section        0  irq_redirect .o(i.I2C0_IRQn_Handler)
    i.I2C1_IRQn_Handler                      0x00010e10   Section        0  irq_redirect .o(i.I2C1_IRQn_Handler)
    i.LCDC_IRQn_Handler                      0x00010e28   Section        0  irq_redirect .o(i.LCDC_IRQn_Handler)
    i.LOG_printf                             0x00010e40   Section        0  tau_log.o(i.LOG_printf)
    i.MEMC_IRQn_Handler                      0x00010e68   Section        0  irq_redirect .o(i.MEMC_IRQn_Handler)
    i.MIPI_RX_IRQn_Handler                   0x00010e80   Section        0  irq_redirect .o(i.MIPI_RX_IRQn_Handler)
    i.MIPI_TX_IRQn_Handler                   0x00010e98   Section        0  irq_redirect .o(i.MIPI_TX_IRQn_Handler)
    i.PWMDET_IRQn_Handler                    0x00010eb0   Section        0  irq_redirect .o(i.PWMDET_IRQn_Handler)
    i.SPIM_IRQn_Handler                      0x00010ecc   Section        0  irq_redirect .o(i.SPIM_IRQn_Handler)
    i.SPIS_IRQn_Handler                      0x00010ee8   Section        0  irq_redirect .o(i.SPIS_IRQn_Handler)
    i.SWIRE_IRQn_Handler                     0x00010f04   Section        0  irq_redirect .o(i.SWIRE_IRQn_Handler)
    i.SysTick_Handler                        0x00010f20   Section        0  irq_redirect .o(i.SysTick_Handler)
    i.TIMER0_IRQn_Handler                    0x00010f38   Section        0  irq_redirect .o(i.TIMER0_IRQn_Handler)
    i.TIMER1_IRQn_Handler                    0x00010f50   Section        0  irq_redirect .o(i.TIMER1_IRQn_Handler)
    i.TIMER2_IRQn_Handler                    0x00010f68   Section        0  irq_redirect .o(i.TIMER2_IRQn_Handler)
    i.TIMER3_IRQn_Handler                    0x00010f80   Section        0  irq_redirect .o(i.TIMER3_IRQn_Handler)
    i.UART0_IRQ_Handle                       0x00010f98   Section        0  drv_uart.o(i.UART0_IRQ_Handle)
    i.UART_DisableDma                        0x00010fb4   Section        0  drv_uart.o(i.UART_DisableDma)
    i.UART_GetInstance                       0x00010fb6   Section        0  drv_uart.o(i.UART_GetInstance)
    i.UART_IRQn_Handler                      0x00010fbc   Section        0  irq_redirect .o(i.UART_IRQn_Handler)
    i.UART_ResetRxFIFO                       0x00010fd4   Section        0  drv_uart.o(i.UART_ResetRxFIFO)
    i.__scatterload_null                     0x00010ff8   Section        2  handlers.o(i.__scatterload_null)
    i.app_tp_screen_int_lvl_low              0x00010ffa   Section        0  app_tp_transfer.o(i.app_tp_screen_int_lvl_low)
    app_tp_screen_int_lvl_low                0x00010ffb   Thumb Code     4  app_tp_transfer.o(i.app_tp_screen_int_lvl_low)
    .ARM.__at_0x11000                        0x00011000   Section       20  drv_common.o(.ARM.__at_0x11000)
    i.drv_dsi_rx_set_inten                   0x00011014   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    .ARM.__at_0x11018                        0x00011018   Section        4  drv_common.o(.ARM.__at_0x11018)
    i.UART_SetBaudRate                       0x0001101c   Section        0  drv_uart.o(i.UART_SetBaudRate)
    i.UART_SwitchSCLK                        0x00011064   Section        0  drv_uart.o(i.UART_SwitchSCLK)
    i.UART_TransferHandleIRQ                 0x0001107e   Section        0  drv_uart.o(i.UART_TransferHandleIRQ)
    i.UART_WriteBlocking                     0x000111b2   Section        0  drv_uart.o(i.UART_WriteBlocking)
    i.UART_init                              0x000111cc   Section        0  drv_uart.o(i.UART_init)
    i.VIDC_IRQn_Handler                      0x00011288   Section        0  irq_redirect .o(i.VIDC_IRQn_Handler)
    i.VPRE_IRQn_Handler                      0x000112a0   Section        0  irq_redirect .o(i.VPRE_IRQn_Handler)
    i.WDG_IRQn_Handler                       0x000112b8   Section        0  irq_redirect .o(i.WDG_IRQn_Handler)
    i.__0printf                              0x000112d0   Section        0  printfa.o(i.__0printf)
    i.__0vsprintf                            0x000112f0   Section        0  printfa.o(i.__0vsprintf)
    i.__ARM_clz                              0x00011314   Section        0  depilogue.o(i.__ARM_clz)
    i.__ARM_common_switch8                   0x00011342   Section        0  hal_dsi_rx_ctrl.o(i.__ARM_common_switch8)
    i.__NVIC_ClearPendingIRQ                 0x0001135c   Section        0  drv_i2c_master.o(i.__NVIC_ClearPendingIRQ)
    __NVIC_ClearPendingIRQ                   0x0001135d   Thumb Code    18  drv_i2c_master.o(i.__NVIC_ClearPendingIRQ)
    i.__NVIC_ClearPendingIRQ                 0x00011374   Section        0  drv_spi_master.o(i.__NVIC_ClearPendingIRQ)
    __NVIC_ClearPendingIRQ                   0x00011375   Thumb Code    18  drv_spi_master.o(i.__NVIC_ClearPendingIRQ)
    i.__NVIC_DisableIRQ                      0x0001138c   Section        0  drv_rxbr.o(i.__NVIC_DisableIRQ)
    __NVIC_DisableIRQ                        0x0001138d   Thumb Code    26  drv_rxbr.o(i.__NVIC_DisableIRQ)
    i.__NVIC_EnableIRQ                       0x000113ac   Section        0  drv_rxbr.o(i.__NVIC_EnableIRQ)
    __NVIC_EnableIRQ                         0x000113ad   Thumb Code    18  drv_rxbr.o(i.__NVIC_EnableIRQ)
    i.__NVIC_SetPriority                     0x000113c4   Section        0  hal_spi_slave.o(i.__NVIC_SetPriority)
    __NVIC_SetPriority                       0x000113c5   Thumb Code    60  hal_spi_slave.o(i.__NVIC_SetPriority)
    i.__NVIC_SystemReset                     0x00011408   Section        0  ap_demo.o(i.__NVIC_SystemReset)
    __NVIC_SystemReset                       0x00011409   Thumb Code    44  ap_demo.o(i.__NVIC_SystemReset)
    i.__scatterload_copy                     0x0001143c   Section       14  handlers.o(i.__scatterload_copy)
    i.__scatterload_zeroinit                 0x0001144a   Section       14  handlers.o(i.__scatterload_zeroinit)
    i.__set_errno                            0x00011458   Section        0  errno.o(i.__set_errno)
    i._fp_digits                             0x00011464   Section        0  printfa.o(i._fp_digits)
    _fp_digits                               0x00011465   Thumb Code   344  printfa.o(i._fp_digits)
    i._printf_core                           0x000115d8   Section        0  printfa.o(i._printf_core)
    _printf_core                             0x000115d9   Thumb Code  1754  printfa.o(i._printf_core)
    i._printf_post_padding                   0x00011cc4   Section        0  printfa.o(i._printf_post_padding)
    _printf_post_padding                     0x00011cc5   Thumb Code    32  printfa.o(i._printf_post_padding)
    i._printf_pre_padding                    0x00011ce4   Section        0  printfa.o(i._printf_pre_padding)
    _printf_pre_padding                      0x00011ce5   Thumb Code    44  printfa.o(i._printf_pre_padding)
    i._sputc                                 0x00011d10   Section        0  printfa.o(i._sputc)
    _sputc                                   0x00011d11   Thumb Code    10  printfa.o(i._sputc)
    i.ap_dcs_read                            0x00011d1c   Section        0  ap_demo.o(i.ap_dcs_read)
    ap_dcs_read                              0x00011d1d   Thumb Code  1184  ap_demo.o(i.ap_dcs_read)
    i.ap_demo                                0x000121bc   Section        0  ap_demo.o(i.ap_demo)
    i.ap_get_51_reg                          0x00012434   Section        0  ap_demo.o(i.ap_get_51_reg)
    ap_get_51_reg                            0x00012435   Thumb Code   182  ap_demo.o(i.ap_get_51_reg)
    i.ap_get_67_reg                          0x00012504   Section        0  ap_demo.o(i.ap_get_67_reg)
    ap_get_67_reg                            0x00012505   Thumb Code    90  ap_demo.o(i.ap_get_67_reg)
    i.ap_get_dcs                             0x00012568   Section        0  ap_demo.o(i.ap_get_dcs)
    ap_get_dcs                               0x00012569   Thumb Code    46  ap_demo.o(i.ap_get_dcs)
    i.ap_get_tp_calibration_status_01        0x0001259c   Section        0  app_tp_st_touch.o(i.ap_get_tp_calibration_status_01)
    i.ap_reset_cb                            0x000125d4   Section        0  ap_demo.o(i.ap_reset_cb)
    ap_reset_cb                              0x000125d5   Thumb Code    40  ap_demo.o(i.ap_reset_cb)
    i.ap_set_display_off                     0x00012610   Section        0  ap_demo.o(i.ap_set_display_off)
    ap_set_display_off                       0x00012611   Thumb Code    40  ap_demo.o(i.ap_set_display_off)
    i.ap_set_display_on                      0x00012664   Section        0  ap_demo.o(i.ap_set_display_on)
    ap_set_display_on                        0x00012665   Thumb Code    24  ap_demo.o(i.ap_set_display_on)
    i.ap_set_enter_sleep_mode                0x000126a4   Section        0  ap_demo.o(i.ap_set_enter_sleep_mode)
    ap_set_enter_sleep_mode                  0x000126a5   Thumb Code    90  ap_demo.o(i.ap_set_enter_sleep_mode)
    i.ap_set_exit_sleep_mode                 0x00012740   Section        0  ap_demo.o(i.ap_set_exit_sleep_mode)
    ap_set_exit_sleep_mode                   0x00012741   Thumb Code    28  ap_demo.o(i.ap_set_exit_sleep_mode)
    i.ap_set_tp_calibration_04               0x00012790   Section        0  app_tp_st_touch.o(i.ap_set_tp_calibration_04)
    i.ap_tp_st_touch_calibration             0x0001285c   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_calibration)
    i.ap_tp_st_touch_error_handler_F3        0x00012924   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_F3)
    i.ap_tp_st_touch_error_handler_FF        0x00012934   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_FF)
    i.ap_tp_st_touch_get_calibration_success_mark 0x00012958   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark)
    i.ap_tp_st_touch_hardware_reset          0x00012a0c   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset)
    i.ap_tp_st_touch_scan_point_init         0x00012ae0   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init)
    i.ap_tp_st_touch_scan_point_record_event 0x00012b04   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event)
    i.ap_tp_st_touch_scan_point_record_event_exec 0x00012bc8   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec)
    i.ap_tp_st_touch_simulate_finger_release_event 0x00012c28   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event)
    i.app_ADC_IRQn_Handler                   0x00012c64   Section        0  drv_rxbr.o(i.app_ADC_IRQn_Handler)
    i.app_AP_NRESET_IRQn_Handler             0x00012c80   Section        0  drv_gpio.o(i.app_AP_NRESET_IRQn_Handler)
    i.app_EXTI_INT0_IRQn_Handler             0x00012ca4   Section        0  drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler)
    i.app_EXTI_INT1_IRQn_Handler             0x00012cc0   Section        0  drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler)
    i.app_EXTI_INT2_IRQn_Handler             0x00012cdc   Section        0  drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler)
    i.app_EXTI_INT3_IRQn_Handler             0x00012cf8   Section        0  drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler)
    i.app_EXTI_INT4_IRQn_Handler             0x00012d14   Section        0  drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler)
    i.app_EXTI_INT5_IRQn_Handler             0x00012d30   Section        0  drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler)
    i.app_EXTI_INT6_IRQn_Handler             0x00012d4c   Section        0  drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler)
    i.app_EXTI_INT7_IRQn_Handler             0x00012d68   Section        0  drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler)
    i.app_HardFault_Handler                  0x00012d84   Section        0  drv_common.o(i.app_HardFault_Handler)
    i.app_I2C0_IRQn_Handler                  0x00012dcc   Section        0  drv_i2c_slave.o(i.app_I2C0_IRQn_Handler)
    i.app_I2C1_IRQn_Handler                  0x00012de4   Section        0  drv_i2c_master.o(i.app_I2C1_IRQn_Handler)
    i.app_LCDC_IRQn_Handler                  0x00012df4   Section        0  hal_internal_vsync.o(i.app_LCDC_IRQn_Handler)
    i.app_MEMC_IRQn_Handler                  0x00012f24   Section        0  drv_memc.o(i.app_MEMC_IRQn_Handler)
    i.app_MIPI_RX_IRQn_Handler               0x00012fac   Section        0  drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler)
    i.app_MIPI_TX_IRQn_Handler               0x00013244   Section        0  drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler)
    i.app_PWMDET_IRQn_Handler                0x000132e4   Section        0  drv_pwm.o(i.app_PWMDET_IRQn_Handler)
    i.app_SPIM_IRQn_Handler                  0x0001332c   Section        0  drv_spi_master.o(i.app_SPIM_IRQn_Handler)
    i.app_SPIS_IRQn_Handler                  0x0001335c   Section        0  hal_spi_slave.o(i.app_SPIS_IRQn_Handler)
    i.app_SWIRE_IRQn_Handler                 0x0001355c   Section        0  drv_swire.o(i.app_SWIRE_IRQn_Handler)
    i.app_SysTick_Handler                    0x0001357c   Section        0  drv_common.o(i.app_SysTick_Handler)
    i.app_TIMER0_IRQn_Handler                0x00013594   Section        0  drv_timer.o(i.app_TIMER0_IRQn_Handler)
    i.app_TIMER1_IRQn_Handler                0x0001359e   Section        0  drv_timer.o(i.app_TIMER1_IRQn_Handler)
    i.app_TIMER2_IRQn_Handler                0x000135a8   Section        0  drv_timer.o(i.app_TIMER2_IRQn_Handler)
    i.app_TIMER3_IRQn_Handler                0x000135b2   Section        0  drv_timer.o(i.app_TIMER3_IRQn_Handler)
    i.app_UART_IRQn_Handler                  0x000135bc   Section        0  drv_uart.o(i.app_UART_IRQn_Handler)
    i.app_VIDC_IRQn_Handler                  0x000135c4   Section        0  drv_vidc.o(i.app_VIDC_IRQn_Handler)
    i.app_VPRE_IRQn_Handler                  0x000135e0   Section        0  drv_rxbr.o(i.app_VPRE_IRQn_Handler)
    i.app_WDG_IRQn_Handler                   0x000135fc   Section        0  drv_wdg.o(i.app_WDG_IRQn_Handler)
    i.app_dma_irq_handler                    0x00013634   Section        0  drv_dma.o(i.app_dma_irq_handler)
    i.app_fls_ctrl_Handler                   0x00013644   Section        0  norflash.o(i.app_fls_ctrl_Handler)
    i.app_tp_calibration_exec                0x00013674   Section        0  app_tp_st_touch.o(i.app_tp_calibration_exec)
    i.app_tp_i2cs_callback                   0x0001372c   Section        0  app_tp_transfer.o(i.app_tp_i2cs_callback)
    app_tp_i2cs_callback                     0x0001372d   Thumb Code    14  app_tp_transfer.o(i.app_tp_i2cs_callback)
    i.app_tp_init                            0x0001373c   Section        0  app_tp_transfer.o(i.app_tp_init)
    i.app_tp_m_read                          0x000137b8   Section        0  app_tp_transfer.o(i.app_tp_m_read)
    i.app_tp_m_transfer_complate             0x000137e8   Section        0  app_tp_transfer.o(i.app_tp_m_transfer_complate)
    i.app_tp_m_write                         0x000137f0   Section        0  app_tp_transfer.o(i.app_tp_m_write)
    i.app_tp_phone_analysis_data             0x00013800   Section        0  app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data)
    i.app_tp_phone_clear_reset_on            0x00013ac0   Section        0  app_tp_transfer.o(i.app_tp_phone_clear_reset_on)
    i.app_tp_s_read                          0x00013acc   Section        0  app_tp_transfer.o(i.app_tp_s_read)
    i.app_tp_s_write                         0x00013adc   Section        0  app_tp_transfer.o(i.app_tp_s_write)
    i.app_tp_screen_analysis_int             0x00013aec   Section        0  app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int)
    i.app_tp_screen_init                     0x00013d6c   Section        0  app_tp_transfer.o(i.app_tp_screen_init)
    i.app_tp_screen_int_callback             0x00013da0   Section        0  app_tp_transfer.o(i.app_tp_screen_int_callback)
    app_tp_screen_int_callback               0x00013da1   Thumb Code     8  app_tp_transfer.o(i.app_tp_screen_int_callback)
    i.app_tp_screen_int_init                 0x00013dac   Section        0  app_tp_transfer.o(i.app_tp_screen_int_init)
    app_tp_screen_int_init                   0x00013dad   Thumb Code    56  app_tp_transfer.o(i.app_tp_screen_int_init)
    i.app_tp_transfer_phone                  0x00013dec   Section        0  app_tp_transfer.o(i.app_tp_transfer_phone)
    app_tp_transfer_phone                    0x00013ded   Thumb Code    48  app_tp_transfer.o(i.app_tp_transfer_phone)
    i.app_tp_transfer_screen_const           0x00013e20   Section        0  app_tp_transfer.o(i.app_tp_transfer_screen_const)
    app_tp_transfer_screen_const             0x00013e21   Thumb Code   280  app_tp_transfer.o(i.app_tp_transfer_screen_const)
    i.app_tp_transfer_screen_int             0x00013f5c   Section        0  app_tp_transfer.o(i.app_tp_transfer_screen_int)
    i.app_tp_transfer_screen_start           0x000140d0   Section        0  app_tp_transfer.o(i.app_tp_transfer_screen_start)
    i.blue_change_ccm                        0x000140dc   Section        0  ap_demo.o(i.blue_change_ccm)
    i.board_Init                             0x00014118   Section        0  board.o(i.board_Init)
    i.calc_framebuffer_setting               0x0001413c   Section        0  hal_internal_vsync.o(i.calc_framebuffer_setting)
    i.ceil                                   0x000146c8   Section        0  ceil.o(i.ceil)
    i.check_mipi_rx_tx_video_info            0x00014790   Section        0  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    check_mipi_rx_tx_video_info              0x00014791   Thumb Code    44  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    i.check_pkt_buf_rev                      0x000147bc   Section        0  hal_internal_vsync.o(i.check_pkt_buf_rev)
    check_pkt_buf_rev                        0x000147bd   Thumb Code    74  hal_internal_vsync.o(i.check_pkt_buf_rev)
    i.dcs_packet_fifo_alloc                  0x00014840   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    i.dcs_packet_fifo_init                   0x00014898   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    i.dcs_packet_free_fifo_header            0x000148b0   Section        0  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    i.dcs_packet_get_fifo_header             0x000148f4   Section        0  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    i.dcs_sw_filter                          0x00014918   Section        0  hal_internal_vsync.o(i.dcs_sw_filter)
    dcs_sw_filter                            0x00014919   Thumb Code    36  hal_internal_vsync.o(i.dcs_sw_filter)
    i.delayMs                                0x00014944   Section        0  tau_delay.o(i.delayMs)
    i.delayUs                                0x0001495c   Section        0  tau_delay.o(i.delayUs)
    i.drv_ap_rst_trig_edge_detect            0x00014980   Section        0  drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect)
    i.drv_chip_info_get_info                 0x000149b8   Section        0  drv_chip_info.o(i.drv_chip_info_get_info)
    i.drv_chip_info_init                     0x000149c4   Section        0  drv_chip_info.o(i.drv_chip_info_init)
    i.drv_chip_rx_info_check                 0x00014a04   Section        0  drv_chip_info.o(i.drv_chip_rx_info_check)
    i.drv_chip_rx_init_done                  0x00014ab4   Section        0  drv_chip_info.o(i.drv_chip_rx_init_done)
    i.drv_common_enable_systick              0x00014ac8   Section        0  drv_common.o(i.drv_common_enable_systick)
    i.drv_common_system_init                 0x00014b20   Section        0  drv_common.o(i.drv_common_system_init)
    i.drv_crgu_config_reset_modules          0x00014b28   Section        0  drv_crgu.o(i.drv_crgu_config_reset_modules)
    i.drv_crgu_set_ahb_pre_div               0x00014b38   Section        0  drv_crgu.o(i.drv_crgu_set_ahb_pre_div)
    i.drv_crgu_set_ahb_src                   0x00014b4c   Section        0  drv_crgu.o(i.drv_crgu_set_ahb_src)
    i.drv_crgu_set_clock                     0x00014b60   Section        0  drv_crgu.o(i.drv_crgu_set_clock)
    i.drv_crgu_set_dpi_mux_src               0x00014b80   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_mux_src)
    i.drv_crgu_set_dpi_pre_div               0x00014b94   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_pre_div)
    i.drv_crgu_set_dpi_pre_src               0x00014bac   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_pre_src)
    i.drv_crgu_set_dsc_core_div              0x00014bc0   Section        0  drv_crgu.o(i.drv_crgu_set_dsc_core_div)
    i.drv_crgu_set_dsco_src                  0x00014bd4   Section        0  drv_crgu.o(i.drv_crgu_set_dsco_src)
    i.drv_crgu_set_dsco_src_div              0x00014be8   Section        0  drv_crgu.o(i.drv_crgu_set_dsco_src_div)
    i.drv_crgu_set_fb_div                    0x00014bfc   Section        0  drv_crgu.o(i.drv_crgu_set_fb_div)
    i.drv_crgu_set_fb_src                    0x00014c10   Section        0  drv_crgu.o(i.drv_crgu_set_fb_src)
    i.drv_crgu_set_lcdc_div                  0x00014c24   Section        0  drv_crgu.o(i.drv_crgu_set_lcdc_div)
    i.drv_crgu_set_lcdc_src                  0x00014c38   Section        0  drv_crgu.o(i.drv_crgu_set_lcdc_src)
    i.drv_crgu_set_mipi_cfg_src              0x00014c4c   Section        0  drv_crgu.o(i.drv_crgu_set_mipi_cfg_src)
    i.drv_crgu_set_mipi_ref_src              0x00014c60   Section        0  drv_crgu.o(i.drv_crgu_set_mipi_ref_src)
    i.drv_crgu_set_reset                     0x00014c78   Section        0  drv_crgu.o(i.drv_crgu_set_reset)
    i.drv_crgu_set_rxbr_div                  0x00014c90   Section        0  drv_crgu.o(i.drv_crgu_set_rxbr_div)
    i.drv_crgu_set_rxbr_src                  0x00014ca4   Section        0  drv_crgu.o(i.drv_crgu_set_rxbr_src)
    i.drv_crgu_set_vidc_src                  0x00014cb8   Section        0  drv_crgu.o(i.drv_crgu_set_vidc_src)
    i.drv_dma_clear_flag                     0x00014ccc   Section        0  drv_dma.o(i.drv_dma_clear_flag)
    i.drv_dma_create_handle                  0x00014ce4   Section        0  drv_dma.o(i.drv_dma_create_handle)
    i.drv_dma_disenable_channel              0x00014d00   Section        0  drv_dma.o(i.drv_dma_disenable_channel)
    i.drv_dma_enable_channel                 0x00014d10   Section        0  drv_dma.o(i.drv_dma_enable_channel)
    i.drv_dma_enable_channel_interrupts      0x00014d20   Section        0  drv_dma.o(i.drv_dma_enable_channel_interrupts)
    i.drv_dma_get_channel_flag               0x00014d44   Section        0  drv_dma.o(i.drv_dma_get_channel_flag)
    i.drv_dma_irq_handler                    0x00014d50   Section        0  drv_dma.o(i.drv_dma_irq_handler)
    i.drv_dma_prepar_transfer                0x00014de0   Section        0  drv_dma.o(i.drv_dma_prepar_transfer)
    i.drv_dma_set_burst                      0x00014df2   Section        0  drv_dma.o(i.drv_dma_set_burst)
    i.drv_dma_set_callback                   0x00014e0c   Section        0  drv_dma.o(i.drv_dma_set_callback)
    i.drv_dma_set_transfer                   0x00014e14   Section        0  drv_dma.o(i.drv_dma_set_transfer)
    i.drv_dsc_dec_convert_pps_rc_parameter   0x00014e58   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter)
    i.drv_dsc_dec_disable                    0x00014e8e   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    i.drv_dsc_dec_enable                     0x00014e9c   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    i.drv_dsc_dec_get_nslc                   0x00014f10   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    i.drv_dsc_dec_set_u8_pps                 0x00014f1a   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps)
    i.drv_dsi_rx_calc_ipi_tx_delay           0x00014f44   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    i.drv_dsi_rx_enable_irq                  0x00015048   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    i.drv_dsi_rx_get_bta_status              0x00015088   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_bta_status)
    i.drv_dsi_rx_get_color_bpp               0x00015098   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    drv_dsi_rx_get_color_bpp                 0x00015099   Thumb Code    62  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    i.drv_dsi_rx_get_color_pcc               0x000150e8   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    drv_dsi_rx_get_color_pcc                 0x000150e9   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    i.drv_dsi_rx_get_compression_en          0x00015104   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    i.drv_dsi_rx_get_max_ret_size            0x0001510c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size)
    i.drv_dsi_rx_power_up                    0x00015112   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    i.drv_dsi_rx_set_ctrl_cfg                0x00015120   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    i.drv_dsi_rx_set_ddi_cfg                 0x00015140   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    i.drv_dsi_rx_set_ipi_cfg                 0x00015150   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    i.drv_dsi_rx_set_lane_swap               0x00015160   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    i.drv_dsi_rx_set_resp_cnt                0x000151a6   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    i.drv_dsi_rx_set_up_phy                  0x000151cc   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    i.drv_dsi_rx_shut_down                   0x000152d0   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    i.drv_dsi_tx_command_header              0x000152de   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    i.drv_dsi_tx_command_mode_cfg            0x000152f2   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    i.drv_dsi_tx_command_put_payload         0x0001535e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    i.drv_dsi_tx_config_eotp                 0x00015362   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    i.drv_dsi_tx_config_int                  0x0001537a   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    i.drv_dsi_tx_dpi_lpcmd_time              0x00015382   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    i.drv_dsi_tx_dpi_mode                    0x0001538a   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    i.drv_dsi_tx_dpi_polarity                0x00015394   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    i.drv_dsi_tx_edpi_cmd_size               0x000153b8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    i.drv_dsi_tx_get_cmd_status              0x000153bc   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    i.drv_dsi_tx_mode                        0x000153c0   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    i.drv_dsi_tx_phy_clock_lane_auto_lp      0x000153c4   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    i.drv_dsi_tx_phy_clock_lane_req_hs       0x000153dc   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    i.drv_dsi_tx_phy_lane_mode               0x000153f6   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    i.drv_dsi_tx_phy_status_ready            0x00015402   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    i.drv_dsi_tx_phy_status_stopstate        0x00015466   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    i.drv_dsi_tx_phy_test_setup              0x000154a4   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    i.drv_dsi_tx_phy_time_cfg                0x000155d8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    i.drv_dsi_tx_powerup                     0x000155f6   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    i.drv_dsi_tx_response_mode               0x000155fe   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    i.drv_dsi_tx_set_bta_ack                 0x0001561a   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    i.drv_dsi_tx_set_esc_div                 0x00015632   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    i.drv_dsi_tx_set_int                     0x00015640   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    i.drv_dsi_tx_set_time_out_div            0x00015680   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    i.drv_dsi_tx_set_video_chunk             0x00015690   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    i.drv_dsi_tx_set_video_timing            0x00015698   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    i.drv_dsi_tx_shutdown                    0x000156ba   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    i.drv_dsi_tx_timeout_cfg                 0x000156c2   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    i.drv_dsi_tx_video_mode_cfg              0x000156e8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    i.drv_dsi_tx_video_mode_disable_hact_cmd 0x00015792   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_disable_hact_cmd)
    i.drv_dsi_tx_video_mode_set_lp_cmd       0x000157a8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd)
    i.drv_efuse_enter_inactive               0x000157c0   Section        0  drv_efuse.o(i.drv_efuse_enter_inactive)
    i.drv_efuse_int_enable                   0x000157ee   Section        0  drv_efuse.o(i.drv_efuse_int_enable)
    i.drv_efuse_read                         0x000157fa   Section        0  drv_efuse.o(i.drv_efuse_read)
    i.drv_efuse_read_req                     0x0001582c   Section        0  drv_efuse.o(i.drv_efuse_read_req)
    i.drv_gpio_get_input_data                0x00015844   Section        0  drv_gpio.o(i.drv_gpio_get_input_data)
    i.drv_gpio_register_ap_reset_callback    0x0001585c   Section        0  drv_gpio.o(i.drv_gpio_register_ap_reset_callback)
    i.drv_gpio_register_callback             0x00015868   Section        0  drv_gpio.o(i.drv_gpio_register_callback)
    i.drv_gpio_set_int                       0x0001587c   Section        0  drv_gpio.o(i.drv_gpio_set_int)
    i.drv_gpio_set_ioe                       0x000158cc   Section        0  drv_gpio.o(i.drv_gpio_set_ioe)
    i.drv_gpio_set_mode0                     0x000158ec   Section        0  drv_gpio.o(i.drv_gpio_set_mode0)
    i.drv_gpio_set_mode1                     0x000158fc   Section        0  drv_gpio.o(i.drv_gpio_set_mode1)
    i.drv_gpio_set_mode2                     0x0001590c   Section        0  drv_gpio.o(i.drv_gpio_set_mode2)
    i.drv_gpio_set_mode3                     0x0001591c   Section        0  drv_gpio.o(i.drv_gpio_set_mode3)
    i.drv_gpio_set_output_data               0x0001592c   Section        0  hal_gpio.o(i.drv_gpio_set_output_data)
    drv_gpio_set_output_data                 0x0001592d   Thumb Code    26  hal_gpio.o(i.drv_gpio_set_output_data)
    i.drv_gpio_set_pull_state                0x0001594c   Section        0  drv_gpio.o(i.drv_gpio_set_pull_state)
    i.drv_i2c0_set_callback                  0x00015a7c   Section        0  drv_i2c_slave.o(i.drv_i2c0_set_callback)
    i.drv_i2c1_set_callback                  0x00015a88   Section        0  drv_i2c_master.o(i.drv_i2c1_set_callback)
    i.drv_i2c_dma_callback                   0x00015a94   Section        0  drv_i2c_dma.o(i.drv_i2c_dma_callback)
    drv_i2c_dma_callback                     0x00015a95   Thumb Code    40  drv_i2c_dma.o(i.drv_i2c_dma_callback)
    i.drv_i2c_dma_init                       0x00015ac8   Section        0  drv_i2c_dma.o(i.drv_i2c_dma_init)
    i.drv_i2c_enable_rx_dma                  0x00015b74   Section        0  drv_i2c_dma.o(i.drv_i2c_enable_rx_dma)
    i.drv_i2c_enable_tx_dma                  0x00015b8e   Section        0  drv_i2c_dma.o(i.drv_i2c_enable_tx_dma)
    i.drv_i2c_m_clear_it_pending_bit         0x00015ba8   Section        0  drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit)
    i.drv_i2c_m_enable                       0x00015c08   Section        0  drv_i2c_master.o(i.drv_i2c_m_enable)
    i.drv_i2c_m_enable_intr                  0x00015c18   Section        0  drv_i2c_master.o(i.drv_i2c_m_enable_intr)
    i.drv_i2c_master_init                    0x00015c50   Section        0  drv_i2c_master.o(i.drv_i2c_master_init)
    i.drv_i2c_master_read_dma                0x00015cdc   Section        0  drv_i2c_dma.o(i.drv_i2c_master_read_dma)
    i.drv_i2c_master_write_dma               0x00015d38   Section        0  drv_i2c_dma.o(i.drv_i2c_master_write_dma)
    i.drv_i2c_master_write_read_cmd          0x00015d74   Section        0  drv_i2c_dma.o(i.drv_i2c_master_write_read_cmd)
    drv_i2c_master_write_read_cmd            0x00015d75   Thumb Code    62  drv_i2c_dma.o(i.drv_i2c_master_write_read_cmd)
    i.drv_i2c_s_clear_it_pending_bit         0x00015db2   Section        0  drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit)
    i.drv_i2c_s_config_intr                  0x00015df4   Section        0  drv_i2c_slave.o(i.drv_i2c_s_config_intr)
    i.drv_i2c_s_enable                       0x00015df8   Section        0  drv_i2c_slave.o(i.drv_i2c_s_enable)
    i.drv_i2c_s_get_fifo_status              0x00015e00   Section        0  drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status)
    i.drv_i2c_s_set_intr                     0x00015e14   Section        0  drv_i2c_slave.o(i.drv_i2c_s_set_intr)
    i.drv_i2c_s_write_data                   0x00015e64   Section        0  drv_i2c_slave.o(i.drv_i2c_s_write_data)
    i.drv_i2c_set_dma_irq_callback           0x00015e80   Section        0  drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback)
    i.drv_i2c_slave_init                     0x00015ed8   Section        0  drv_i2c_slave.o(i.drv_i2c_slave_init)
    i.drv_i2c_slave_write_dma                0x00015f0c   Section        0  drv_i2c_dma.o(i.drv_i2c_slave_write_dma)
    i.drv_lcdc_config_bypass                 0x00015f24   Section        0  drv_lcdc.o(i.drv_lcdc_config_bypass)
    i.drv_lcdc_config_ccm                    0x00015f3c   Section        0  drv_lcdc.o(i.drv_lcdc_config_ccm)
    i.drv_lcdc_config_disp_mode              0x00015f6c   Section        0  drv_lcdc.o(i.drv_lcdc_config_disp_mode)
    i.drv_lcdc_config_dpi_polarity           0x00015f82   Section        0  drv_lcdc.o(i.drv_lcdc_config_dpi_polarity)
    i.drv_lcdc_config_dpi_timing             0x00015fa6   Section        0  drv_lcdc.o(i.drv_lcdc_config_dpi_timing)
    i.drv_lcdc_config_edpi_mode              0x00015fcc   Section        0  drv_lcdc.o(i.drv_lcdc_config_edpi_mode)
    i.drv_lcdc_config_endianness             0x00015fe2   Section        0  drv_lcdc.o(i.drv_lcdc_config_endianness)
    i.drv_lcdc_config_input_size             0x00015ff8   Section        0  drv_lcdc.o(i.drv_lcdc_config_input_size)
    i.drv_lcdc_config_int                    0x00016004   Section        0  drv_lcdc.o(i.drv_lcdc_config_int)
    i.drv_lcdc_config_int_single             0x00016022   Section        0  drv_lcdc.o(i.drv_lcdc_config_int_single)
    i.drv_lcdc_config_overwrite              0x00016044   Section        0  drv_lcdc.o(i.drv_lcdc_config_overwrite)
    i.drv_lcdc_config_overwrite_rgb          0x00016066   Section        0  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    i.drv_lcdc_config_partial_display_area   0x00016072   Section        0  drv_lcdc.o(i.drv_lcdc_config_partial_display_area)
    i.drv_lcdc_config_partial_display_enable 0x0001608c   Section        0  drv_lcdc.o(i.drv_lcdc_config_partial_display_enable)
    i.drv_lcdc_config_scale_up_coef          0x000160ae   Section        0  drv_lcdc.o(i.drv_lcdc_config_scale_up_coef)
    i.drv_lcdc_config_scale_up_step          0x000160c8   Section        0  drv_lcdc.o(i.drv_lcdc_config_scale_up_step)
    i.drv_lcdc_config_src_parameter          0x000160d4   Section        0  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    i.drv_lcdc_config_thresh                 0x00016120   Section        0  drv_lcdc.o(i.drv_lcdc_config_thresh)
    i.drv_lcdc_ctrl_flow                     0x00016126   Section        0  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    i.drv_lcdc_enable_shadow_reg             0x00016138   Section        0  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    i.drv_lcdc_set_int                       0x00016158   Section        0  drv_lcdc.o(i.drv_lcdc_set_int)
    i.drv_lcdc_set_prefetch                  0x00016198   Section        0  drv_lcdc.o(i.drv_lcdc_set_prefetch)
    i.drv_lcdc_set_video_hw_mode             0x000161b0   Section        0  drv_lcdc.o(i.drv_lcdc_set_video_hw_mode)
    i.drv_lcdc_start                         0x000161c4   Section        0  drv_lcdc.o(i.drv_lcdc_start)
    i.drv_memc_clear_status                  0x000161e4   Section        0  drv_memc.o(i.drv_memc_clear_status)
    i.drv_memc_enable_irq                    0x000161f0   Section        0  drv_memc.o(i.drv_memc_enable_irq)
    i.drv_memc_gen_a_tear_signal             0x00016230   Section        0  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    i.drv_memc_get_status                    0x0001623c   Section        0  drv_memc.o(i.drv_memc_get_status)
    i.drv_memc_rate_transfer_sel             0x0001624e   Section        0  drv_memc.o(i.drv_memc_rate_transfer_sel)
    i.drv_memc_sel_vsync                     0x0001625e   Section        0  drv_memc.o(i.drv_memc_sel_vsync)
    i.drv_memc_set_active_height             0x0001626c   Section        0  drv_memc.o(i.drv_memc_set_active_height)
    i.drv_memc_set_data_mode                 0x00016280   Section        0  drv_memc.o(i.drv_memc_set_data_mode)
    i.drv_memc_set_double_buffer             0x0001628c   Section        0  drv_memc.o(i.drv_memc_set_double_buffer)
    i.drv_memc_set_double_buffer_reverse     0x0001629c   Section        0  drv_memc.o(i.drv_memc_set_double_buffer_reverse)
    i.drv_memc_set_fs_en_conditions          0x000162ae   Section        0  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    i.drv_memc_set_inten                     0x000162be   Section        0  drv_memc.o(i.drv_memc_set_inten)
    i.drv_memc_set_lcdc_st_conditions        0x000162d4   Section        0  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    i.drv_memc_set_ltpo_mode                 0x000162ec   Section        0  drv_memc.o(i.drv_memc_set_ltpo_mode)
    i.drv_memc_set_tear_mode                 0x00016306   Section        0  drv_memc.o(i.drv_memc_set_tear_mode)
    i.drv_memc_set_tear_waveform             0x00016314   Section        0  drv_memc.o(i.drv_memc_set_tear_waveform)
    i.drv_memc_set_vidc_sync_cnt             0x0001633c   Section        0  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    i.drv_param_init_get_ccm                 0x0001634c   Section        0  drv_param_init.o(i.drv_param_init_get_ccm)
    i.drv_param_init_get_scld_filter_h       0x00016354   Section        0  drv_param_init.o(i.drv_param_init_get_scld_filter_h)
    i.drv_param_init_get_scld_filter_v       0x00016368   Section        0  drv_param_init.o(i.drv_param_init_get_scld_filter_v)
    i.drv_param_init_get_sclu_filter         0x0001637c   Section        0  drv_param_init.o(i.drv_param_init_get_sclu_filter)
    i.drv_param_init_set_ccm                 0x00016384   Section        0  drv_param_init.o(i.drv_param_init_set_ccm)
    i.drv_param_init_set_scld_filter         0x00016398   Section        0  drv_param_init.o(i.drv_param_init_set_scld_filter)
    i.drv_param_p2r_filter_init              0x000163fc   Section        0  drv_param_init.o(i.drv_param_p2r_filter_init)
    i.drv_phy_enable_calibration             0x00016420   Section        0  drv_phy_common.o(i.drv_phy_enable_calibration)
    i.drv_phy_get_calibration                0x00016430   Section        0  drv_phy_common.o(i.drv_phy_get_calibration)
    i.drv_phy_get_pll_para                   0x0001646c   Section        0  drv_phy_common.o(i.drv_phy_get_pll_para)
    i.drv_phy_get_rate_para                  0x000164cc   Section        0  drv_phy_common.o(i.drv_phy_get_rate_para)
    i.drv_phy_test_clear                     0x00016520   Section        0  drv_phy_common.o(i.drv_phy_test_clear)
    i.drv_phy_test_lock                      0x00016530   Section        0  drv_phy_common.o(i.drv_phy_test_lock)
    i.drv_phy_test_write_1_byte              0x00016548   Section        0  drv_phy_common.o(i.drv_phy_test_write_1_byte)
    i.drv_phy_test_write_2_byte              0x00016568   Section        0  drv_phy_common.o(i.drv_phy_test_write_2_byte)
    i.drv_phy_test_write_code                0x0001658e   Section        0  drv_phy_common.o(i.drv_phy_test_write_code)
    i.drv_phy_test_write_data                0x000165ac   Section        0  drv_phy_common.o(i.drv_phy_test_write_data)
    drv_phy_test_write_data                  0x000165ad   Thumb Code    32  drv_phy_common.o(i.drv_phy_test_write_data)
    i.drv_pwr_set_cp_mode                    0x000165cc   Section        0  drv_pwr.o(i.drv_pwr_set_cp_mode)
    i.drv_pwr_set_pvd_mode                   0x000165ec   Section        0  drv_pwr.o(i.drv_pwr_set_pvd_mode)
    i.drv_pwr_set_system_clk_src             0x00016604   Section        0  drv_pwr.o(i.drv_pwr_set_system_clk_src)
    i.drv_rx_phy_test_clear                  0x0001663c   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_clear)
    drv_rx_phy_test_clear                    0x0001663d   Thumb Code    12  drv_dsi_rx.o(i.drv_rx_phy_test_clear)
    i.drv_rx_phy_test_lock                   0x00016648   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_lock)
    drv_rx_phy_test_lock                     0x00016649   Thumb Code    16  drv_dsi_rx.o(i.drv_rx_phy_test_lock)
    i.drv_rx_phy_test_write_1_byte           0x00016658   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte)
    drv_rx_phy_test_write_1_byte             0x00016659   Thumb Code    20  drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte)
    i.drv_rx_phy_test_write_2_byte           0x0001666c   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte)
    drv_rx_phy_test_write_2_byte             0x0001666d   Thumb Code    22  drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte)
    i.drv_rxbr_clear_pkt_buffer              0x00016682   Section        0  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    i.drv_rxbr_clear_status0                 0x0001668c   Section        0  drv_rxbr.o(i.drv_rxbr_clear_status0)
    i.drv_rxbr_enable_irq                    0x00016690   Section        0  drv_rxbr.o(i.drv_rxbr_enable_irq)
    i.drv_rxbr_frame_drop_cfg                0x000166ec   Section        0  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    i.drv_rxbr_get_clk                       0x00016700   Section        0  drv_rxbr.o(i.drv_rxbr_get_clk)
    i.drv_rxbr_get_col_addr                  0x00016764   Section        0  drv_rxbr.o(i.drv_rxbr_get_col_addr)
    i.drv_rxbr_get_int_source                0x00016768   Section        0  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    drv_rxbr_get_int_source                  0x00016769   Thumb Code    18  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    i.drv_rxbr_get_page_addr                 0x0001677a   Section        0  drv_rxbr.o(i.drv_rxbr_get_page_addr)
    i.drv_rxbr_get_pkt_buf_error_status      0x0001677e   Section        0  drv_rxbr.o(i.drv_rxbr_get_pkt_buf_error_status)
    i.drv_rxbr_get_status0                   0x0001678a   Section        0  hal_internal_vsync.o(i.drv_rxbr_get_status0)
    drv_rxbr_get_status0                     0x0001678b   Thumb Code    18  hal_internal_vsync.o(i.drv_rxbr_get_status0)
    i.drv_rxbr_get_status1                   0x0001679c   Section        0  hal_internal_vsync.o(i.drv_rxbr_get_status1)
    drv_rxbr_get_status1                     0x0001679d   Thumb Code    22  hal_internal_vsync.o(i.drv_rxbr_get_status1)
    i.drv_rxbr_hline_rcv1_cfg                0x000167b2   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg)
    i.drv_rxbr_hline_rcv_cfg                 0x000167be   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    i.drv_rxbr_register_irq0_callback        0x000167c8   Section        0  drv_rxbr.o(i.drv_rxbr_register_irq0_callback)
    i.drv_rxbr_register_irq1_callback        0x000167d4   Section        0  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    i.drv_rxbr_set_ack_pkt_header            0x000167e0   Section        0  drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header)
    i.drv_rxbr_set_color_format              0x000167f4   Section        0  drv_rxbr.o(i.drv_rxbr_set_color_format)
    i.drv_rxbr_set_filter_regs               0x00016808   Section        0  drv_rxbr.o(i.drv_rxbr_set_filter_regs)
    i.drv_rxbr_set_inten                     0x0001681a   Section        0  drv_rxbr.o(i.drv_rxbr_set_inten)
    i.drv_rxbr_set_ltpo_drop_th              0x0001682e   Section        0  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    i.drv_rxbr_set_usr_cfg                   0x0001683e   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    i.drv_rxbr_set_usr_col                   0x00016864   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    i.drv_rxbr_set_usr_row                   0x0001686c   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    i.drv_spi_m_read_data                    0x00016874   Section        0  drv_spi_master.o(i.drv_spi_m_read_data)
    i.drv_swire_enable                       0x00016894   Section        0  drv_swire.o(i.drv_swire_enable)
    i.drv_swire_set_int                      0x000168b0   Section        0  drv_swire.o(i.drv_swire_set_int)
    i.drv_swire_set_power_down               0x00016904   Section        0  drv_swire.o(i.drv_swire_set_power_down)
    i.drv_sys_cfg_clear_all_int              0x00016920   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    i.drv_sys_cfg_clear_pending              0x0001692c   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    i.drv_sys_cfg_sel_ap_rst_lvl_trig        0x00016954   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig)
    i.drv_sys_cfg_sel_ap_rst_trig            0x0001696c   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig)
    i.drv_sys_cfg_sel_gpio_group             0x00016988   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group)
    i.drv_sys_cfg_sel_int_trig               0x000169ac   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig)
    i.drv_sys_cfg_set_dma_rx_req             0x000169d0   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req)
    i.drv_sys_cfg_set_dma_tx_req             0x000169e0   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req)
    i.drv_sys_cfg_set_int                    0x000169f0   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    i.drv_timer_clear_status_flags           0x00016a14   Section        0  drv_timer.o(i.drv_timer_clear_status_flags)
    drv_timer_clear_status_flags             0x00016a15   Thumb Code    26  drv_timer.o(i.drv_timer_clear_status_flags)
    i.drv_timer_enable                       0x00016a2e   Section        0  drv_timer.o(i.drv_timer_enable)
    i.drv_timer_get_instance                 0x00016a50   Section        0  drv_timer.o(i.drv_timer_get_instance)
    i.drv_timer_get_prescaler                0x00016a60   Section        0  drv_timer.o(i.drv_timer_get_prescaler)
    i.drv_timer_handle_interrupt             0x00016a70   Section        0  drv_timer.o(i.drv_timer_handle_interrupt)
    drv_timer_handle_interrupt               0x00016a71   Thumb Code    62  drv_timer.o(i.drv_timer_handle_interrupt)
    i.drv_timer_register_callback            0x00016ab4   Section        0  drv_timer.o(i.drv_timer_register_callback)
    i.drv_timer_set_compare_val              0x00016ac8   Section        0  drv_timer.o(i.drv_timer_set_compare_val)
    i.drv_timer_set_int                      0x00016ad8   Section        0  drv_timer.o(i.drv_timer_set_int)
    i.drv_timer_set_prescaler                0x00016b2c   Section        0  drv_timer.o(i.drv_timer_set_prescaler)
    i.drv_timer_set_repeat                   0x00016b54   Section        0  drv_timer.o(i.drv_timer_set_repeat)
    i.drv_tx_phy_test_clear                  0x00016b64   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_clear)
    drv_tx_phy_test_clear                    0x00016b65   Thumb Code    10  drv_dsi_tx.o(i.drv_tx_phy_test_clear)
    i.drv_tx_phy_test_enter                  0x00016b6e   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    i.drv_tx_phy_test_exit                   0x00016b8a   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    i.drv_tx_phy_test_write_1_byte           0x00016ba6   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte)
    drv_tx_phy_test_write_1_byte             0x00016ba7   Thumb Code    18  drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte)
    i.drv_tx_phy_test_write_2_byte           0x00016bb8   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte)
    drv_tx_phy_test_write_2_byte             0x00016bb9   Thumb Code    20  drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte)
    i.drv_tx_phy_test_write_code             0x00016bcc   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    drv_tx_phy_test_write_code               0x00016bcd   Thumb Code    16  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    i.drv_vidc_clear_irq                     0x00016bdc   Section        0  drv_vidc.o(i.drv_vidc_clear_irq)
    i.drv_vidc_enable                        0x00016be4   Section        0  drv_vidc.o(i.drv_vidc_enable)
    i.drv_vidc_enable_irq                    0x00016bfc   Section        0  drv_vidc.o(i.drv_vidc_enable_irq)
    i.drv_vidc_get_irq_status                0x00016c3c   Section        0  drv_vidc.o(i.drv_vidc_get_irq_status)
    i.drv_vidc_init_module_enable            0x00016c50   Section        0  drv_vidc.o(i.drv_vidc_init_module_enable)
    i.drv_vidc_register_callback             0x00016c78   Section        0  drv_vidc.o(i.drv_vidc_register_callback)
    i.drv_vidc_reset                         0x00016c84   Section        0  drv_vidc.o(i.drv_vidc_reset)
    i.drv_vidc_set_dst_parameter             0x00016c8a   Section        0  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    i.drv_vidc_set_irqen                     0x00016cc6   Section        0  drv_vidc.o(i.drv_vidc_set_irqen)
    i.drv_vidc_set_mirror                    0x00016cda   Section        0  drv_vidc.o(i.drv_vidc_set_mirror)
    i.drv_vidc_set_p2r_hcoef0                0x00016cea   Section        0  drv_vidc.o(i.drv_vidc_set_p2r_hcoef0)
    i.drv_vidc_set_p2r_hinitb                0x00016cf2   Section        0  drv_vidc.o(i.drv_vidc_set_p2r_hinitb)
    i.drv_vidc_set_p2r_hinitr                0x00016d18   Section        0  drv_vidc.o(i.drv_vidc_set_p2r_hinitr)
    i.drv_vidc_set_pentile_swap              0x00016d40   Section        0  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    i.drv_vidc_set_pu_ctrl                   0x00016d58   Section        0  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    i.drv_vidc_set_rotation                  0x00016d62   Section        0  drv_vidc.o(i.drv_vidc_set_rotation)
    i.drv_vidc_set_scld_hcoef0               0x00016d72   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    i.drv_vidc_set_scld_hcoef1               0x00016d7c   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    i.drv_vidc_set_scld_step                 0x00016d86   Section        0  drv_vidc.o(i.drv_vidc_set_scld_step)
    i.drv_vidc_set_scld_vcoef0               0x00016d98   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    i.drv_vidc_set_scld_vcoef1               0x00016da2   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    i.drv_vidc_set_src_parameter             0x00016dac   Section        0  drv_vidc.o(i.drv_vidc_set_src_parameter)
    i.drv_wdg_clear_counter                  0x00016dc4   Section        0  drv_wdg.o(i.drv_wdg_clear_counter)
    i.drv_wdg_clear_edge_flag                0x00016dd4   Section        0  drv_wdg.o(i.drv_wdg_clear_edge_flag)
    drv_wdg_clear_edge_flag                  0x00016dd5   Thumb Code    12  drv_wdg.o(i.drv_wdg_clear_edge_flag)
    i.drv_wdg_read_edge_flag                 0x00016de4   Section        0  drv_wdg.o(i.drv_wdg_read_edge_flag)
    drv_wdg_read_edge_flag                   0x00016de5   Thumb Code    10  drv_wdg.o(i.drv_wdg_read_edge_flag)
    i.drv_wdg_set_int                        0x00016df4   Section        0  drv_wdg.o(i.drv_wdg_set_int)
    i.finger_calibration_init                0x00016e34   Section        0  ap_demo.o(i.finger_calibration_init)
    i.fls_clr_interrupt_flag                 0x00016e48   Section        0  drv_fls.o(i.fls_clr_interrupt_flag)
    i.fputc                                  0x00016e52   Section        0  tau_log.o(i.fputc)
    i.hal_dsi_rx_ctrl_ack_long_cmd           0x00016e68   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd)
    i.hal_dsi_rx_ctrl_create_handle          0x00016ec0   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    i.hal_dsi_rx_ctrl_deinit                 0x00016ef4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit)
    i.hal_dsi_rx_ctrl_dsc_async_handler      0x00016fa4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler)
    i.hal_dsi_rx_ctrl_gen_a_tear_signal      0x00016fcc   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal)
    i.hal_dsi_rx_ctrl_get_max_ret_size       0x00016ff4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size)
    i.hal_dsi_rx_ctrl_init                   0x0001701c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    i.hal_dsi_rx_ctrl_init_clk               0x000170b4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    hal_dsi_rx_ctrl_init_clk                 0x000170b5   Thumb Code   332  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    i.hal_dsi_rx_ctrl_init_dsi_rx            0x00017258   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    hal_dsi_rx_ctrl_init_dsi_rx              0x00017259   Thumb Code   184  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    i.hal_dsi_rx_ctrl_init_memc              0x00017330   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    hal_dsi_rx_ctrl_init_memc                0x00017331   Thumb Code   342  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    i.hal_dsi_rx_ctrl_init_rxbr              0x00017490   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    hal_dsi_rx_ctrl_init_rxbr                0x00017491   Thumb Code   320  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    i.hal_dsi_rx_ctrl_init_vidc              0x000175e0   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    hal_dsi_rx_ctrl_init_vidc                0x000175e1   Thumb Code   544  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    i.hal_dsi_rx_ctrl_pre_init_pps           0x0001780c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    i.hal_dsi_rx_ctrl_send_ack_cmd           0x00017848   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd)
    i.hal_dsi_rx_ctrl_set_cus_scld_filter    0x00017938   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter)
    i.hal_dsi_rx_ctrl_set_hw_tear_mode       0x000179a4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode)
    i.hal_dsi_rx_ctrl_set_ipi_cfg            0x000179d8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    hal_dsi_rx_ctrl_set_ipi_cfg              0x000179d9   Thumb Code    50  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    i.hal_dsi_rx_ctrl_set_rxbr_clk           0x00017a10   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk)
    hal_dsi_rx_ctrl_set_rxbr_clk             0x00017a11   Thumb Code   114  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk)
    i.hal_dsi_rx_ctrl_set_sw_tear_mode       0x00017a84   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode)
    i.hal_dsi_rx_ctrl_set_tear_mode_ex       0x00017ab8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex)
    i.hal_dsi_rx_ctrl_start                  0x00017ac8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    i.hal_dsi_rx_ctrl_stop                   0x00017b04   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop)
    i.hal_dsi_rx_ctrl_toggle_resolution      0x00017b40   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    i.hal_dsi_tx_calc_video_chunks           0x00017b60   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks)
    hal_dsi_tx_calc_video_chunks             0x00017b61   Thumb Code   384  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks)
    i.hal_dsi_tx_config_params_for_lane_rate 0x00017cf0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate)
    hal_dsi_tx_config_params_for_lane_rate   0x00017cf1   Thumb Code    42  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate)
    i.hal_dsi_tx_count_lane_rate             0x00017d24   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate)
    hal_dsi_tx_count_lane_rate               0x00017d25   Thumb Code   982  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate)
    i.hal_dsi_tx_ctrl_create_handle          0x0001814c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    i.hal_dsi_tx_ctrl_deinit                 0x00018178   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit)
    i.hal_dsi_tx_ctrl_enter_init_panel_mode  0x000181fc   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode)
    i.hal_dsi_tx_ctrl_exit_init_panel_mode   0x00018248   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode)
    i.hal_dsi_tx_ctrl_init                   0x00018270   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    i.hal_dsi_tx_ctrl_init_clk               0x00018314   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    hal_dsi_tx_ctrl_init_clk                 0x00018315   Thumb Code    36  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    i.hal_dsi_tx_ctrl_panel_reset_pin        0x00018338   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin)
    i.hal_dsi_tx_ctrl_set_ccm                0x00018344   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm)
    i.hal_dsi_tx_ctrl_set_overwrite_rgb      0x00018364   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    i.hal_dsi_tx_ctrl_set_partial_disp       0x00018378   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp)
    i.hal_dsi_tx_ctrl_set_partial_disp_area  0x00018388   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area)
    i.hal_dsi_tx_ctrl_start                  0x000183ac   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    i.hal_dsi_tx_ctrl_stop                   0x00018454   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop)
    i.hal_dsi_tx_ctrl_write_cmd              0x00018498   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    i.hal_dsi_tx_init_data_mode              0x00018564   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode)
    hal_dsi_tx_init_data_mode                0x00018565   Thumb Code    58  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode)
    i.hal_dsi_tx_init_dpi_cfg                0x000185a8   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg)
    hal_dsi_tx_init_dpi_cfg                  0x000185a9   Thumb Code    42  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg)
    i.hal_dsi_tx_init_interrupt              0x000185d8   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt)
    hal_dsi_tx_init_interrupt                0x000185d9   Thumb Code    28  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt)
    i.hal_dsi_tx_init_phy_cfg                0x000185f8   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    hal_dsi_tx_init_phy_cfg                  0x000185f9   Thumb Code    28  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    i.hal_dsi_tx_init_remains                0x00018618   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains)
    hal_dsi_tx_init_remains                  0x00018619   Thumb Code   142  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains)
    i.hal_dsi_tx_init_video_mode             0x000186ac   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode)
    hal_dsi_tx_init_video_mode               0x000186ad   Thumb Code    82  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode)
    i.hal_dsi_tx_send_cmd                    0x00018704   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    hal_dsi_tx_send_cmd                      0x00018705   Thumb Code    60  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    i.hal_gpio_ctrl_eint                     0x00018748   Section        0  hal_gpio.o(i.hal_gpio_ctrl_eint)
    i.hal_gpio_get_input_data                0x00018760   Section        0  hal_gpio.o(i.hal_gpio_get_input_data)
    i.hal_gpio_init_eint                     0x00018774   Section        0  hal_gpio.o(i.hal_gpio_init_eint)
    i.hal_gpio_init_input                    0x000187b4   Section        0  hal_gpio.o(i.hal_gpio_init_input)
    i.hal_gpio_init_output                   0x000187d4   Section        0  hal_gpio.o(i.hal_gpio_init_output)
    i.hal_gpio_reg_eint_cb                   0x000187fc   Section        0  hal_gpio.o(i.hal_gpio_reg_eint_cb)
    i.hal_gpio_set_ap_reset_int              0x00018814   Section        0  hal_gpio.o(i.hal_gpio_set_ap_reset_int)
    i.hal_gpio_set_mode                      0x00018864   Section        0  hal_gpio.o(i.hal_gpio_set_mode)
    i.hal_gpio_set_output_data               0x000188c4   Section        0  hal_gpio.o(i.hal_gpio_set_output_data)
    i.hal_gpio_set_pull_state                0x000188cc   Section        0  hal_gpio.o(i.hal_gpio_set_pull_state)
    i.hal_i2c_m_dma_init                     0x000188ec   Section        0  hal_i2c_master.o(i.hal_i2c_m_dma_init)
    i.hal_i2c_m_dma_read                     0x00018958   Section        0  hal_i2c_master.o(i.hal_i2c_m_dma_read)
    i.hal_i2c_m_dma_write                    0x00018978   Section        0  hal_i2c_master.o(i.hal_i2c_m_dma_write)
    i.hal_i2c_m_transfer_complate            0x00018994   Section        0  hal_i2c_master.o(i.hal_i2c_m_transfer_complate)
    i.hal_i2c_master_irq_callback            0x000189a0   Section        0  hal_i2c_master.o(i.hal_i2c_master_irq_callback)
    hal_i2c_master_irq_callback              0x000189a1   Thumb Code    24  hal_i2c_master.o(i.hal_i2c_master_irq_callback)
    i.hal_i2c_s_dma_user_callback            0x000189c0   Section        0  hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback)
    hal_i2c_s_dma_user_callback              0x000189c1   Thumb Code    12  hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback)
    i.hal_i2c_s_dma_write                    0x000189d0   Section        0  hal_i2c_slave.o(i.hal_i2c_s_dma_write)
    i.hal_i2c_s_init                         0x00018a1c   Section        0  hal_i2c_slave.o(i.hal_i2c_s_init)
    i.hal_i2c_s_nonblocking_read             0x00018ae4   Section        0  hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read)
    i.hal_i2c_s_set_transfer                 0x00018af8   Section        0  hal_i2c_slave.o(i.hal_i2c_s_set_transfer)
    i.hal_i2c_slave_irq_callback             0x00018b04   Section        0  hal_i2c_slave.o(i.hal_i2c_slave_irq_callback)
    hal_i2c_slave_irq_callback               0x00018b05   Thumb Code   356  hal_i2c_slave.o(i.hal_i2c_slave_irq_callback)
    i.hal_internal_check_video_auto_sync     0x00018c78   Section        0  hal_internal_vsync.o(i.hal_internal_check_video_auto_sync)
    i.hal_internal_init_memc                 0x00018c90   Section        0  hal_internal_vsync.o(i.hal_internal_init_memc)
    i.hal_internal_rx_dcs_async_handler      0x00018d8c   Section        0  hal_internal_vsync.o(i.hal_internal_rx_dcs_async_handler)
    i.hal_internal_rx_dcs_polling            0x00018db8   Section        0  hal_internal_vsync.o(i.hal_internal_rx_dcs_polling)
    i.hal_internal_sync_get_fb_setting       0x00018e10   Section        0  hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting)
    i.hal_internal_sync_get_hight_performan_mode 0x00018e20   Section        0  hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode)
    i.hal_internal_sync_input_resolution_change 0x00018e30   Section        0  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    i.hal_internal_vsync_deinit              0x0001905c   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    i.hal_internal_vsync_get_rx_state        0x00019084   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state)
    i.hal_internal_vsync_get_sync_line       0x00019090   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    i.hal_internal_vsync_get_tear_mode       0x000190a8   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_tear_mode)
    i.hal_internal_vsync_get_tx_state        0x000190b4   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    i.hal_internal_vsync_init_rx             0x000190c0   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    i.hal_internal_vsync_init_tx             0x00019200   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    i.hal_internal_vsync_set_auto_hw_filter  0x000192b0   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter)
    i.hal_internal_vsync_set_rx_state        0x00019340   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    i.hal_internal_vsync_set_tear_mode       0x00019364   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    i.hal_internal_vsync_set_tx_state        0x000193b4   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    i.hal_intl_svs_deinit_tx                 0x00019438   Section        0  hal_internal_soft_sync.o(i.hal_intl_svs_deinit_tx)
    i.hal_intl_svs_handle                    0x00019448   Section        0  hal_internal_soft_sync.o(i.hal_intl_svs_handle)
    i.hal_intl_svs_init_rx                   0x0001946c   Section        0  hal_internal_soft_sync.o(i.hal_intl_svs_init_rx)
    i.hal_intl_svs_init_tx                   0x000194e4   Section        0  hal_internal_soft_sync.o(i.hal_intl_svs_init_tx)
    i.hal_intl_svs_update_rxbr_clk           0x000194f8   Section        0  hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk)
    i.hal_lcdc_config_ccm                    0x00019540   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm)
    hal_lcdc_config_ccm                      0x00019541   Thumb Code    30  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm)
    i.hal_lcdc_config_remains                0x00019564   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains)
    hal_lcdc_config_remains                  0x00019565   Thumb Code    94  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains)
    i.hal_lcdc_config_rgb_to_pentile         0x000195c8   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile)
    hal_lcdc_config_rgb_to_pentile           0x000195c9   Thumb Code    14  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile)
    i.hal_lcdc_config_upscaler               0x000195dc   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler)
    hal_lcdc_config_upscaler                 0x000195dd   Thumb Code   348  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler)
    i.hal_lcdc_init_cfg                      0x00019740   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    hal_lcdc_init_cfg                        0x00019741   Thumb Code    78  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    i.hal_lcdc_init_clk                      0x00019794   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    hal_lcdc_init_clk                        0x00019795   Thumb Code   446  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    i.hal_lcdc_init_interrupt                0x00019960   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt)
    hal_lcdc_init_interrupt                  0x00019961   Thumb Code    58  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt)
    i.hal_spi_m_clear_rxfifo                 0x000199a0   Section        0  hal_spi_master.o(i.hal_spi_m_clear_rxfifo)
    i.hal_swire_deinit                       0x000199ae   Section        0  hal_swire.o(i.hal_swire_deinit)
    i.hal_swire_open                         0x000199c0   Section        0  hal_swire.o(i.hal_swire_open)
    i.hal_system_enable_systick              0x000199d6   Section        0  hal_system.o(i.hal_system_enable_systick)
    i.hal_system_init                        0x000199e0   Section        0  hal_system.o(i.hal_system_init)
    i.hal_system_init_console                0x00019a68   Section        0  hal_system.o(i.hal_system_init_console)
    i.hal_system_set_phy_calibration         0x00019a84   Section        0  hal_system.o(i.hal_system_set_phy_calibration)
    i.hal_system_set_pvd                     0x00019a8c   Section        0  hal_system.o(i.hal_system_set_pvd)
    i.hal_system_set_vcc                     0x00019a94   Section        0  hal_system.o(i.hal_system_set_vcc)
    i.hal_timer_deinit                       0x00019a9c   Section        0  hal_timer.o(i.hal_timer_deinit)
    i.hal_timer_init                         0x00019aca   Section        0  hal_timer.o(i.hal_timer_init)
    i.hal_timer_start                        0x00019ae4   Section        0  hal_timer.o(i.hal_timer_start)
    i.hal_timer_stop                         0x00019b2c   Section        0  hal_timer.o(i.hal_timer_stop)
    i.hal_tx_frame_rate_adjust               0x00019b54   Section        0  hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust)
    hal_tx_frame_rate_adjust                 0x00019b55   Thumb Code    44  hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust)
    i.hal_uart_init                          0x00019b84   Section        0  hal_uart.o(i.hal_uart_init)
    i.hal_uart_transmit_blocking             0x00019c10   Section        0  hal_uart.o(i.hal_uart_transmit_blocking)
    i.handle_init                            0x00019c20   Section        0  irq_redirect .o(i.handle_init)
    i.init_mipi_tx                           0x00019d30   Section        0  ap_demo.o(i.init_mipi_tx)
    init_mipi_tx                             0x00019d31   Thumb Code   174  ap_demo.o(i.init_mipi_tx)
    i.init_panel                             0x00019de8   Section        0  ap_demo.o(i.init_panel)
    init_panel                               0x00019de9   Thumb Code 10838  ap_demo.o(i.init_panel)
    i.main                                   0x0001c83e   Section        0  main.o(i.main)
    i.open_mipi_rx                           0x0001c850   Section        0  ap_demo.o(i.open_mipi_rx)
    open_mipi_rx                             0x0001c851   Thumb Code   258  ap_demo.o(i.open_mipi_rx)
    i.pps_update_handle                      0x0001c978   Section        0  ap_demo.o(i.pps_update_handle)
    pps_update_handle                        0x0001c979   Thumb Code    98  ap_demo.o(i.pps_update_handle)
    i.rx_get_dcs_packet_data                 0x0001ca10   Section        0  hal_internal_vsync.o(i.rx_get_dcs_packet_data)
    rx_get_dcs_packet_data                   0x0001ca11   Thumb Code   654  hal_internal_vsync.o(i.rx_get_dcs_packet_data)
    i.rx_partial_update                      0x0001ce04   Section        0  hal_internal_vsync.o(i.rx_partial_update)
    rx_partial_update                        0x0001ce05   Thumb Code   348  hal_internal_vsync.o(i.rx_partial_update)
    i.rx_receive_packet                      0x0001cf70   Section        0  hal_internal_vsync.o(i.rx_receive_packet)
    rx_receive_packet                        0x0001cf71   Thumb Code   126  hal_internal_vsync.o(i.rx_receive_packet)
    i.rx_receive_pps                         0x0001cffc   Section        0  hal_internal_vsync.o(i.rx_receive_pps)
    rx_receive_pps                           0x0001cffd   Thumb Code   268  hal_internal_vsync.o(i.rx_receive_pps)
    i.rxbr_irq0_callback                     0x0001d17c   Section        0  hal_internal_vsync.o(i.rxbr_irq0_callback)
    rxbr_irq0_callback                       0x0001d17d   Thumb Code   192  hal_internal_vsync.o(i.rxbr_irq0_callback)
    i.rxbr_irq1_callback                     0x0001d248   Section        0  hal_internal_vsync.o(i.rxbr_irq1_callback)
    rxbr_irq1_callback                       0x0001d249   Thumb Code   392  hal_internal_vsync.o(i.rxbr_irq1_callback)
    i.set_soft_tear_mode                     0x0001d48c   Section        0  ap_demo.o(i.set_soft_tear_mode)
    set_soft_tear_mode                       0x0001d48d   Thumb Code    44  ap_demo.o(i.set_soft_tear_mode)
    i.soft_gen_te                            0x0001d4c0   Section        0  hal_internal_vsync.o(i.soft_gen_te)
    soft_gen_te                              0x0001d4c1   Thumb Code   166  hal_internal_vsync.o(i.soft_gen_te)
    i.soft_gen_te_double_buffer              0x0001d584   Section        0  hal_internal_vsync.o(i.soft_gen_te_double_buffer)
    soft_gen_te_double_buffer                0x0001d585   Thumb Code   166  hal_internal_vsync.o(i.soft_gen_te_double_buffer)
    i.soft_te_timer_cb                       0x0001d644   Section        0  ap_demo.o(i.soft_te_timer_cb)
    soft_te_timer_cb                         0x0001d645   Thumb Code    44  ap_demo.o(i.soft_te_timer_cb)
    i.soft_te_timer_init                     0x0001d67c   Section        0  ap_demo.o(i.soft_te_timer_init)
    soft_te_timer_init                       0x0001d67d   Thumb Code    30  ap_demo.o(i.soft_te_timer_init)
    i.soft_timer3_cb                         0x0001d6a4   Section        0  ap_demo.o(i.soft_timer3_cb)
    soft_timer3_cb                           0x0001d6a5   Thumb Code    46  ap_demo.o(i.soft_timer3_cb)
    i.sqrt                                   0x0001d6e0   Section        0  sqrt.o(i.sqrt)
    i.svs_direct_mode_setting                0x0001d728   Section        0  hal_internal_soft_sync.o(i.svs_direct_mode_setting)
    svs_direct_mode_setting                  0x0001d729   Thumb Code   156  hal_internal_soft_sync.o(i.svs_direct_mode_setting)
    i.svs_get_rel_intv                       0x0001d7d4   Section        0  hal_internal_soft_sync.o(i.svs_get_rel_intv)
    svs_get_rel_intv                         0x0001d7d5   Thumb Code    20  hal_internal_soft_sync.o(i.svs_get_rel_intv)
    i.svs_sync_handle                        0x0001d7f0   Section        0  hal_internal_soft_sync.o(i.svs_sync_handle)
    svs_sync_handle                          0x0001d7f1   Thumb Code   158  hal_internal_soft_sync.o(i.svs_sync_handle)
    i.svs_wait_start                         0x0001d8a0   Section        0  hal_internal_soft_sync.o(i.svs_wait_start)
    svs_wait_start                           0x0001d8a1   Thumb Code   224  hal_internal_soft_sync.o(i.svs_wait_start)
    i.svs_waite_fr_stab                      0x0001d994   Section        0  hal_internal_soft_sync.o(i.svs_waite_fr_stab)
    svs_waite_fr_stab                        0x0001d995   Thumb Code   148  hal_internal_soft_sync.o(i.svs_waite_fr_stab)
    i.tp_heartbeat_exec                      0x0001da6c   Section        0  ap_demo.o(i.tp_heartbeat_exec)
    i.tx_display_on                          0x0001dac4   Section        0  ap_demo.o(i.tx_display_on)
    tx_display_on                            0x0001dac5   Thumb Code    40  ap_demo.o(i.tx_display_on)
    i.tx_panel_reset                         0x0001daf4   Section        0  ap_demo.o(i.tx_panel_reset)
    tx_panel_reset                           0x0001daf5   Thumb Code    54  ap_demo.o(i.tx_panel_reset)
    i.vidc_callback                          0x0001db60   Section        0  hal_internal_vsync.o(i.vidc_callback)
    vidc_callback                            0x0001db61   Thumb Code   234  hal_internal_vsync.o(i.vidc_callback)
    i.vpre_err_reset                         0x0001dc68   Section        0  hal_internal_vsync.o(i.vpre_err_reset)
    vpre_err_reset                           0x0001dc69   Thumb Code   192  hal_internal_vsync.o(i.vpre_err_reset)
    i.vsync_set_te_mode                      0x0001dd40   Section        0  hal_internal_vsync.o(i.vsync_set_te_mode)
    vsync_set_te_mode                        0x0001dd41   Thumb Code   300  hal_internal_vsync.o(i.vsync_set_te_mode)
    .constdata                               0x0001df0c   Section      376  ap_demo.o(.constdata)
    g_cus_rx_dcs_execute_table               0x0001df0c   Data         108  ap_demo.o(.constdata)
    .constdata                               0x0001e084   Section       32  app_tp_st_touch.o(.constdata)
    .constdata                               0x0001e0a4   Section       36  hal_dsi_tx_ctrl.o(.constdata)
    .constdata                               0x0001e0c8   Section      210  hal_gpio.o(.constdata)
    s_gpio_map                               0x0001e0c8   Data         120  hal_gpio.o(.constdata)
    s_gpio_perf                              0x0001e140   Data          90  hal_gpio.o(.constdata)
    .constdata                               0x0001e19c   Section       32  hal_i2c_slave.o(.constdata)
    sg_i2c_s_config                          0x0001e19c   Data          32  hal_i2c_slave.o(.constdata)
    .constdata                               0x0001e1bc   Section     1622  app_tp_for_custom_s8.o(.constdata)
    .constdata                               0x0001e814   Section        8  drv_param_init.o(.constdata)
    .constdata                               0x0001e81c   Section      390  drv_phy_common.o(.constdata)
    phy_para_mapping_h                       0x0001e81c   Data         184  drv_phy_common.o(.constdata)
    phy_para_mapping_l                       0x0001e8d4   Data         128  drv_phy_common.o(.constdata)
    phy_data_high_map                        0x0001e954   Data          48  drv_phy_common.o(.constdata)
    phy_data_lp_map                          0x0001e984   Data          30  drv_phy_common.o(.constdata)
    .conststring                             0x0001e9a4   Section       80  ap_demo.o(.conststring)
    .conststring                             0x0001e9f4   Section       72  hal_dsi_rx_ctrl.o(.conststring)
    .conststring                             0x0001ea3c   Section       67  hal_dsi_tx_ctrl.o(.conststring)
    .conststring                             0x0001ea80   Section      376  hal_internal_vsync.o(.conststring)
    .ARM.__AT_0x00070100                     0x00070100   Section      192  irq_redirect .o(.ARM.__AT_0x00070100)
    .data                                    0x000701d0   Section      584  ap_demo.o(.data)
    g_rx_ctrl_handle                         0x000701d0   Data           4  ap_demo.o(.data)
    g_tx_ctrl_handle                         0x000701d4   Data           4  ap_demo.o(.data)
    swire_num                                0x000701d8   Data           1  ap_demo.o(.data)
    swire_num_bak                            0x000701d9   Data           1  ap_demo.o(.data)
    g_swire_num                              0x000701da   Data           1  ap_demo.o(.data)
    g_mipi_path_off                          0x000701db   Data           1  ap_demo.o(.data)
    start_display_on                         0x000701dc   Data           1  ap_demo.o(.data)
    g_exit_sleep_mode                        0x000701dd   Data           1  ap_demo.o(.data)
    g_need_enter_sleep_mode                  0x000701de   Data           1  ap_demo.o(.data)
    panel_display_done                       0x000701df   Data           1  ap_demo.o(.data)
    g_resolution_change                      0x000701e0   Data           1  ap_demo.o(.data)
    g_reg51_value_1b8_flag                   0x000701e1   Data           1  ap_demo.o(.data)
    g_calibration_flag                       0x000701e9   Data           1  ap_demo.o(.data)
    rx_filter_1080_h_4_86                    0x000701f4   Data         256  ap_demo.o(.data)
    rx_filter_2340_v_4_95                    0x000702f4   Data         256  ap_demo.o(.data)
    value_reg_df                             0x000703f8   Data           4  ap_demo.o(.data)
    value_blue                               0x000703fc   Data           1  ap_demo.o(.data)
    blue_flag                                0x000703fd   Data           1  ap_demo.o(.data)
    s20_power_on_flag                        0x00070400   Data           4  ap_demo.o(.data)
    s_finger_flag                            0x00070408   Data           1  ap_demo.o(.data)
    value_reg_51                             0x0007040c   Data           4  ap_demo.o(.data)
    lastvalue_reg_51                         0x00070410   Data           4  ap_demo.o(.data)
    value_reg_67                             0x00070414   Data           1  ap_demo.o(.data)
    flag_te                                  0x00070415   Data           1  ap_demo.o(.data)
    reset_pre_high                           0x00070416   Data           1  ap_demo.o(.data)
    need_reset                               0x00070417   Data           1  ap_demo.o(.data)
    .data                                    0x00070418   Section       64  app_tp_transfer.o(.data)
    s_spim_write                             0x00070425   Data           1  app_tp_transfer.o(.data)
    s_screen_int_flag                        0x00070426   Data           1  app_tp_transfer.o(.data)
    s_phone_reset_flag                       0x00070427   Data           1  app_tp_transfer.o(.data)
    s_screen_int_transfer_status             0x00070428   Data           1  app_tp_transfer.o(.data)
    s_screen_const_transfer_count            0x0007042a   Data           1  app_tp_transfer.o(.data)
    screen_int_transfer_count                0x00070456   Data           1  app_tp_transfer.o(.data)
    screen_int_transfer_buffer_ready         0x00070457   Data           1  app_tp_transfer.o(.data)
    .data                                    0x00070458   Section       40  app_tp_st_touch.o(.data)
    s_calibration_flag                       0x00070458   Data           1  app_tp_st_touch.o(.data)
    s_calibration_correct_flag               0x00070459   Data           1  app_tp_st_touch.o(.data)
    .data                                    0x00070480   Section        8  hal_dsi_rx_ctrl.o(.data)
    g_hw_auto_filter                         0x00070480   Data           1  hal_dsi_rx_ctrl.o(.data)
    g_esc_clk                                0x00070484   Data           4  hal_dsi_rx_ctrl.o(.data)
    .data                                    0x00070488   Section        3  hal_dsi_tx_ctrl.o(.data)
    g_tx_vcom_en                             0x00070488   Data           1  hal_dsi_tx_ctrl.o(.data)
    g_tx_vpg_en                              0x00070489   Data           1  hal_dsi_tx_ctrl.o(.data)
    g_tx_mode                                0x0007048a   Data           1  hal_dsi_tx_ctrl.o(.data)
    .data                                    0x0007048b   Section        1  hal_i2c_master.o(.data)
    s_i2c_m_transfer_end                     0x0007048b   Data           1  hal_i2c_master.o(.data)
    .data                                    0x0007048c   Section       32  hal_i2c_slave.o(.data)
    s_txbuffer_complate                      0x0007048c   Data           1  hal_i2c_slave.o(.data)
    s_i2c_s_dma_end                          0x0007048d   Data           1  hal_i2c_slave.o(.data)
    s_i2c_s_receive_cnt                      0x0007048e   Data           1  hal_i2c_slave.o(.data)
    sg_i2c_s_index                           0x0007048f   Data           1  hal_i2c_slave.o(.data)
    s_hal_slave_rxbuffer                     0x00070490   Data           4  hal_i2c_slave.o(.data)
    s_hal_slave_rxbuffer_size                0x00070494   Data           4  hal_i2c_slave.o(.data)
    hal_i2c_s_callback                       0x00070498   Data           4  hal_i2c_slave.o(.data)
    sg_tx_byte_num                           0x0007049c   Data           4  hal_i2c_slave.o(.data)
    s_receive_count                          0x000704a0   Data           4  hal_i2c_slave.o(.data)
    s_tx_buffer_t                            0x000704a4   Data           4  hal_i2c_slave.o(.data)
    tx_sum                                   0x000704a8   Data           4  hal_i2c_slave.o(.data)
    .data                                    0x000704ac   Section      794  app_tp_for_custom_s8.o(.data)
    u16CoordY                                0x000704ca   Data           2  app_tp_for_custom_s8.o(.data)
    u16CoordX                                0x000704cc   Data           2  app_tp_for_custom_s8.o(.data)
    u16CoordY_back                           0x000704ce   Data           2  app_tp_for_custom_s8.o(.data)
    u16CoordX_back                           0x000704d0   Data           2  app_tp_for_custom_s8.o(.data)
    enctryptCnt                              0x000704d8   Data           4  app_tp_for_custom_s8.o(.data)
    app_tp_count                             0x000707c5   Data           1  app_tp_for_custom_s8.o(.data)
    .data                                    0x000707c8   Section       24  hal_internal_vsync.o(.data)
    sg_cmd_mode_tx_start                     0x000707c8   Data           1  hal_internal_vsync.o(.data)
    sg_cur_te_info                           0x000707cc   Data           4  hal_internal_vsync.o(.data)
    g_cus_rx_write_cmd_handle                0x000707d4   Data          12  hal_internal_vsync.o(.data)
    .data                                    0x000707e0   Section       12  drv_common.o(.data)
    s_my_tick                                0x000707e0   Data           4  drv_common.o(.data)
    .data                                    0x000707ec   Section        4  drv_gpio.o(.data)
    g_ap_reset_cb                            0x000707ec   Data           4  drv_gpio.o(.data)
    .data                                    0x000707f0   Section        8  drv_i2c_dma.o(.data)
    i2c0_dma_callback                        0x000707f0   Data           4  drv_i2c_dma.o(.data)
    i2c1_dma_callback                        0x000707f4   Data           4  drv_i2c_dma.o(.data)
    .data                                    0x000707f8   Section        4  drv_i2c_master.o(.data)
    i2c1_intr_callback                       0x000707f8   Data           4  drv_i2c_master.o(.data)
    .data                                    0x000707fc   Section        4  drv_i2c_slave.o(.data)
    i2c0_intr_callback                       0x000707fc   Data           4  drv_i2c_slave.o(.data)
    .data                                    0x00070800   Section     1188  drv_param_init.o(.data)
    .data                                    0x00070ca4   Section        4  drv_spi_master.o(.data)
    SPIM_intr_callback                       0x00070ca4   Data           4  drv_spi_master.o(.data)
    .data                                    0x00070ca8   Section        8  drv_swire.o(.data)
    s_swire_cb                               0x00070ca8   Data           8  drv_swire.o(.data)
    .data                                    0x00070cb0   Section        1  drv_sys_cfg.o(.data)
    sg_ap_rstn_trigger_type                  0x00070cb0   Data           1  drv_sys_cfg.o(.data)
    .data                                    0x00070cb4   Section       80  drv_timer.o(.data)
    sg_timer_info                            0x00070cb4   Data          80  drv_timer.o(.data)
    .data                                    0x00070d04   Section        8  drv_rxbr.o(.data)
    .data                                    0x00070d0c   Section        4  drv_vidc.o(.data)
    .data                                    0x00070d10   Section        1  drv_phy_common.o(.data)
    g_phy_calibration                        0x00070d10   Data           1  drv_phy_common.o(.data)
    .data                                    0x00070d14   Section       12  drv_chip_info.o(.data)
    sg_chip_info                             0x00070d14   Data           4  drv_chip_info.o(.data)
    sg_chip_function                         0x00070d18   Data           4  drv_chip_info.o(.data)
    sg_chip_encrypt                          0x00070d1c   Data           4  drv_chip_info.o(.data)
    .data                                    0x00070d20   Section       18  norflash.o(.data)
    tmprg                                    0x00070d28   Data           4  norflash.o(.data)
    .data                                    0x00070d34   Section       12  drv_pwm.o(.data)
    s_pwm_type                               0x00070d34   Data           1  drv_pwm.o(.data)
    s_pwm_cb                                 0x00070d38   Data           8  drv_pwm.o(.data)
    .data                                    0x00070d40   Section        8  drv_uart.o(.data)
    s_UartFcrReg                             0x00070d40   Data           4  drv_uart.o(.data)
    uart_userData                            0x00070d44   Data           4  drv_uart.o(.data)
    .data                                    0x00070d48   Section       12  drv_wdg.o(.data)
    sg_wdg_repeat                            0x00070d48   Data           1  drv_wdg.o(.data)
    sg_wdg_cb                                0x00070d4c   Data           8  drv_wdg.o(.data)
    .data                                    0x00070d54   Section        4  stdout.o(.data)
    .data                                    0x00070d58   Section        4  errno.o(.data)
    _errno                                   0x00070d58   Data           4  errno.o(.data)
    .bss                                     0x00070d5c   Section      580  app_tp_transfer.o(.bss)
    s_screen_read_buffer                     0x00070dac   Data         200  app_tp_transfer.o(.bss)
    s_phone_read_buffer                      0x00070e74   Data         200  app_tp_transfer.o(.bss)
    .bss                                     0x00070fa0   Section       12  app_tp_st_touch.o(.bss)
    .bss                                     0x00070fac   Section      196  hal_dsi_rx_ctrl.o(.bss)
    g_rx_ctrl_handle_inst                    0x00070fac   Data         196  hal_dsi_rx_ctrl.o(.bss)
    .bss                                     0x00071070   Section       76  hal_dsi_tx_ctrl.o(.bss)
    g_tx_ctrl_handle_inst                    0x00071070   Data          76  hal_dsi_tx_ctrl.o(.bss)
    .bss                                     0x000710bc   Section      256  tau_log.o(.bss)
    .bss                                     0x000711bc   Section      208  hal_uart.o(.bss)
    .bss                                     0x0007128c   Section     2420  hal_internal_vsync.o(.bss)
    g_imm_buffer                             0x00071ae0   Data         255  hal_internal_vsync.o(.bss)
    sg_te_info                               0x00071be0   Data          12  hal_internal_vsync.o(.bss)
    g_imm_packet                             0x00071bec   Data          20  hal_internal_vsync.o(.bss)
    .bss                                     0x00071c00   Section       28  drv_dma.o(.bss)
    s_dma_handle                             0x00071c00   Data          28  drv_dma.o(.bss)
    .bss                                     0x00071c1c   Section       64  drv_gpio.o(.bss)
    s_gpio_cb                                0x00071c1c   Data          64  drv_gpio.o(.bss)
    .bss                                     0x00071c5c   Section      320  drv_i2c_dma.o(.bss)
    i2c0_dma_slave_handle                    0x00071c5c   Data         160  drv_i2c_dma.o(.bss)
    i2c1_dma_master_handle                   0x00071cfc   Data         160  drv_i2c_dma.o(.bss)
    .bss                                     0x00071d9c   Section       64  hal_internal_soft_sync.o(.bss)
    sg_sys_handler                           0x00071d9c   Data          64  hal_internal_soft_sync.o(.bss)
    .bss                                     0x00071ddc   Section       32  hal_spi_slave.o(.bss)
    .bss                                     0x00071dfc   Section     4144  dcs_packet_fifo.o(.bss)
    STACK                                    0x00072e30   Section     4096  startup_armcm0.o(STACK)

    Global Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    BuildAttributes$$THM_ISAv3M$S$PE$A:L22$X:L11$S22$IEEE1$IW$USESV6$~STKCKD$USESV7$~SHL$OTIME$ROPI$IEEEJ$EBA8$MICROLIB$REQ8$PRES8$EABIv2 0x00000000   Number         0  anon$$obj.o ABSOLUTE
    __ARM_use_no_argv                        0x00000000   Number         0  main.o ABSOLUTE
    _printf_a                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_c                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_charcount                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_d                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_e                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_f                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_flags                            0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_dec                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_hex                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_g                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_i                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_int_dec                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_l                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ll                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lld                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lli                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llo                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llu                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llx                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_dec                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_hex                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_oct                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ls                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_mbtowc                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_n                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_o                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_p                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_percent                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_pre_padding                      0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_return_value                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_s                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_sizespec                         0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_str                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_signed                  0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_unsigned                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_u                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wctomb                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_widthprec                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_x                                0x00000000   Number         0  stubs.o ABSOLUTE
    __cpp_initialize__aeabi_                  - Undefined Weak Reference
    __cxa_finalize                            - Undefined Weak Reference
    _clock_init                               - Undefined Weak Reference
    _microlib_exit                            - Undefined Weak Reference
    __Vectors_Size                           0x000000c0   Number         0  startup_armcm0.o ABSOLUTE
    __Vectors                                0x00010000   Data           4  startup_armcm0.o(RESET)
    __Vectors_End                            0x000100c0   Data           0  startup_armcm0.o(RESET)
    __main                                   0x000100c1   Thumb Code     0  entry.o(.ARM.Collect$$$$00000000)
    _main_stk                                0x000100c1   Thumb Code     0  entry2.o(.ARM.Collect$$$$00000001)
    _main_scatterload                        0x000100c5   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    __main_after_scatterload                 0x000100c9   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    _main_clock                              0x000100c9   Thumb Code     0  entry7b.o(.ARM.Collect$$$$00000008)
    _main_cpp_init                           0x000100c9   Thumb Code     0  entry8b.o(.ARM.Collect$$$$0000000A)
    _main_init                               0x000100c9   Thumb Code     0  entry9a.o(.ARM.Collect$$$$0000000B)
    __rt_final_cpp                           0x000100d1   Thumb Code     0  entry10a.o(.ARM.Collect$$$$0000000D)
    __rt_final_exit                          0x000100d1   Thumb Code     0  entry11a.o(.ARM.Collect$$$$0000000F)
    Reset_Handler                            0x000100d5   Thumb Code    28  startup_armcm0.o(.text)
    NMI_Handler                              0x000100f1   Thumb Code     2  startup_armcm0.o(.text)
    SVC_Handler                              0x000100f5   Thumb Code     2  startup_armcm0.o(.text)
    PendSV_Handler                           0x000100f7   Thumb Code     2  startup_armcm0.o(.text)
    OTP_IRQn_Handler                         0x00010123   Thumb Code     2  startup_armcm0.o(.text)
    PVD_IRQn_Handler                         0x00010127   Thumb Code     2  startup_armcm0.o(.text)
    __aeabi_uidiv                            0x0001014d   Thumb Code     0  uidiv.o(.text)
    __aeabi_uidivmod                         0x0001014d   Thumb Code    44  uidiv.o(.text)
    __aeabi_idiv                             0x00010179   Thumb Code     0  idiv.o(.text)
    __aeabi_idivmod                          0x00010179   Thumb Code    40  idiv.o(.text)
    __aeabi_memcpy                           0x000101a1   Thumb Code    36  memcpya.o(.text)
    __aeabi_memcpy4                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memcpy8                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memset                           0x000101c5   Thumb Code    14  memseta.o(.text)
    __aeabi_memset4                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memset8                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr                           0x000101d3   Thumb Code     4  memseta.o(.text)
    __aeabi_memclr4                          0x000101d3   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr8                          0x000101d3   Thumb Code     0  memseta.o(.text)
    _memset$wrapper                          0x000101d7   Thumb Code    18  memseta.o(.text)
    __aeabi_fadd                             0x000101e9   Thumb Code   162  fadd.o(.text)
    __aeabi_fsub                             0x0001028b   Thumb Code     8  fadd.o(.text)
    __aeabi_frsub                            0x00010293   Thumb Code     8  fadd.o(.text)
    __aeabi_fmul                             0x0001029b   Thumb Code   122  fmul.o(.text)
    __aeabi_fdiv                             0x00010315   Thumb Code   124  fdiv.o(.text)
    __ARM_scalbnf                            0x00010391   Thumb Code    24  fscalb.o(.text)
    scalbnf                                  0x00010391   Thumb Code     0  fscalb.o(.text)
    __aeabi_dadd                             0x000103a9   Thumb Code   328  dadd.o(.text)
    __aeabi_dsub                             0x000104f1   Thumb Code    12  dadd.o(.text)
    __aeabi_drsub                            0x000104fd   Thumb Code    12  dadd.o(.text)
    __aeabi_dmul                             0x0001050d   Thumb Code   202  dmul.o(.text)
    __aeabi_ddiv                             0x000105dd   Thumb Code   234  ddiv.o(.text)
    __aeabi_i2f                              0x000106cd   Thumb Code    22  fflti.o(.text)
    __aeabi_ui2f                             0x000106e3   Thumb Code    14  ffltui.o(.text)
    __aeabi_ui2d                             0x000106f1   Thumb Code    24  dfltui.o(.text)
    __aeabi_f2iz                             0x0001070d   Thumb Code    50  ffixi.o(.text)
    __aeabi_f2uiz                            0x0001073f   Thumb Code    40  ffixui.o(.text)
    __aeabi_d2iz                             0x00010769   Thumb Code    62  dfixi.o(.text)
    __aeabi_d2uiz                            0x000107b1   Thumb Code    50  dfixui.o(.text)
    __aeabi_f2d                              0x000107ed   Thumb Code    40  f2d.o(.text)
    __aeabi_cdcmpeq                          0x00010815   Thumb Code     0  cdcmple.o(.text)
    __aeabi_cdcmple                          0x00010815   Thumb Code    38  cdcmple.o(.text)
    __aeabi_cfcmpeq                          0x0001083d   Thumb Code     0  cfcmple.o(.text)
    __aeabi_cfcmple                          0x0001083d   Thumb Code    20  cfcmple.o(.text)
    __aeabi_cfrcmple                         0x00010851   Thumb Code    20  cfrcmple.o(.text)
    __aeabi_uldivmod                         0x00010865   Thumb Code    96  uldiv.o(.text)
    __aeabi_llsl                             0x000108c5   Thumb Code    32  llshl.o(.text)
    _ll_shift_l                              0x000108c5   Thumb Code     0  llshl.o(.text)
    __aeabi_llsr                             0x000108e5   Thumb Code    34  llushr.o(.text)
    _ll_ushift_r                             0x000108e5   Thumb Code     0  llushr.o(.text)
    __aeabi_lasr                             0x00010907   Thumb Code    38  llsshr.o(.text)
    _ll_sshift_r                             0x00010907   Thumb Code     0  llsshr.o(.text)
    __I$use$fp                               0x0001092d   Thumb Code     0  iusefp.o(.text)
    _float_round                             0x0001092d   Thumb Code    16  fepilogue.o(.text)
    _float_epilogue                          0x0001093d   Thumb Code   114  fepilogue.o(.text)
    _double_round                            0x000109af   Thumb Code    26  depilogue.o(.text)
    _double_epilogue                         0x000109c9   Thumb Code   164  depilogue.o(.text)
    _dsqrt                                   0x00010a6d   Thumb Code   162  dsqrt.o(.text)
    __aeabi_d2ulz                            0x00010b11   Thumb Code    54  dfixul.o(.text)
    __aeabi_cdrcmple                         0x00010b51   Thumb Code    38  cdrcmple.o(.text)
    __scatterload                            0x00010b79   Thumb Code    28  init.o(.text)
    __scatterload_rt2                        0x00010b79   Thumb Code     0  init.o(.text)
    __decompress                             0x00010b9d   Thumb Code     0  __dczerorl2.o(.text)
    __decompress1                            0x00010b9d   Thumb Code    86  __dczerorl2.o(.text)
    ADC_IRQn_Handler                         0x00010bf5   Thumb Code    18  irq_redirect .o(i.ADC_IRQn_Handler)
    AP_NRESET_IRQn_Handler                   0x00010c0d   Thumb Code    18  irq_redirect .o(i.AP_NRESET_IRQn_Handler)
    CRC16_2                                  0x00010c25   Thumb Code    62  app_tp_st_touch.o(i.CRC16_2)
    DMA_IRQn_Handler                         0x00010c6d   Thumb Code    14  irq_redirect .o(i.DMA_IRQn_Handler)
    EXTI_INT0_IRQn_Handler                   0x00010c81   Thumb Code    22  irq_redirect .o(i.EXTI_INT0_IRQn_Handler)
    EXTI_INT1_IRQn_Handler                   0x00010c9d   Thumb Code    22  irq_redirect .o(i.EXTI_INT1_IRQn_Handler)
    EXTI_INT2_IRQn_Handler                   0x00010cb9   Thumb Code    22  irq_redirect .o(i.EXTI_INT2_IRQn_Handler)
    EXTI_INT3_IRQn_Handler                   0x00010cd5   Thumb Code    22  irq_redirect .o(i.EXTI_INT3_IRQn_Handler)
    EXTI_INT4_IRQn_Handler                   0x00010cf1   Thumb Code    22  irq_redirect .o(i.EXTI_INT4_IRQn_Handler)
    EXTI_INT5_IRQn_Handler                   0x00010d0d   Thumb Code    22  irq_redirect .o(i.EXTI_INT5_IRQn_Handler)
    EXTI_INT6_IRQn_Handler                   0x00010d29   Thumb Code    22  irq_redirect .o(i.EXTI_INT6_IRQn_Handler)
    EXTI_INT7_IRQn_Handler                   0x00010d45   Thumb Code    22  irq_redirect .o(i.EXTI_INT7_IRQn_Handler)
    EncryptCheck                             0x00010d61   Thumb Code    28  app_tp_for_custom_s8.o(i.EncryptCheck)
    FLSCTRL_IRQn_Handler                     0x00010d81   Thumb Code    14  irq_redirect .o(i.FLSCTRL_IRQn_Handler)
    Gpio_swire_output                        0x00010d95   Thumb Code    80  ap_demo.o(i.Gpio_swire_output)
    HardFault_Handler                        0x00010de5   Thumb Code    14  irq_redirect .o(i.HardFault_Handler)
    I2C0_IRQn_Handler                        0x00010df9   Thumb Code    18  irq_redirect .o(i.I2C0_IRQn_Handler)
    I2C1_IRQn_Handler                        0x00010e11   Thumb Code    18  irq_redirect .o(i.I2C1_IRQn_Handler)
    LCDC_IRQn_Handler                        0x00010e29   Thumb Code    18  irq_redirect .o(i.LCDC_IRQn_Handler)
    LOG_printf                               0x00010e41   Thumb Code    30  tau_log.o(i.LOG_printf)
    MEMC_IRQn_Handler                        0x00010e69   Thumb Code    18  irq_redirect .o(i.MEMC_IRQn_Handler)
    MIPI_RX_IRQn_Handler                     0x00010e81   Thumb Code    18  irq_redirect .o(i.MIPI_RX_IRQn_Handler)
    MIPI_TX_IRQn_Handler                     0x00010e99   Thumb Code    18  irq_redirect .o(i.MIPI_TX_IRQn_Handler)
    PWMDET_IRQn_Handler                      0x00010eb1   Thumb Code    22  irq_redirect .o(i.PWMDET_IRQn_Handler)
    SPIM_IRQn_Handler                        0x00010ecd   Thumb Code    22  irq_redirect .o(i.SPIM_IRQn_Handler)
    SPIS_IRQn_Handler                        0x00010ee9   Thumb Code    22  irq_redirect .o(i.SPIS_IRQn_Handler)
    SWIRE_IRQn_Handler                       0x00010f05   Thumb Code    22  irq_redirect .o(i.SWIRE_IRQn_Handler)
    SysTick_Handler                          0x00010f21   Thumb Code    18  irq_redirect .o(i.SysTick_Handler)
    TIMER0_IRQn_Handler                      0x00010f39   Thumb Code    18  irq_redirect .o(i.TIMER0_IRQn_Handler)
    TIMER1_IRQn_Handler                      0x00010f51   Thumb Code    18  irq_redirect .o(i.TIMER1_IRQn_Handler)
    TIMER2_IRQn_Handler                      0x00010f69   Thumb Code    18  irq_redirect .o(i.TIMER2_IRQn_Handler)
    TIMER3_IRQn_Handler                      0x00010f81   Thumb Code    18  irq_redirect .o(i.TIMER3_IRQn_Handler)
    UART0_IRQ_Handle                         0x00010f99   Thumb Code    20  drv_uart.o(i.UART0_IRQ_Handle)
    UART_DisableDma                          0x00010fb5   Thumb Code     2  drv_uart.o(i.UART_DisableDma)
    UART_GetInstance                         0x00010fb7   Thumb Code     4  drv_uart.o(i.UART_GetInstance)
    UART_IRQn_Handler                        0x00010fbd   Thumb Code    18  irq_redirect .o(i.UART_IRQn_Handler)
    UART_ResetRxFIFO                         0x00010fd5   Thumb Code    32  drv_uart.o(i.UART_ResetRxFIFO)
    __scatterload_null                       0x00010ff9   Thumb Code     2  handlers.o(i.__scatterload_null)
    s_RAM_CK                                 0x00011000   Data          20  drv_common.o(.ARM.__at_0x11000)
    drv_dsi_rx_set_inten                     0x00011015   Thumb Code     4  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    s_debug_state                            0x00011018   Data           4  drv_common.o(.ARM.__at_0x11018)
    UART_SetBaudRate                         0x0001101d   Thumb Code    72  drv_uart.o(i.UART_SetBaudRate)
    UART_SwitchSCLK                          0x00011065   Thumb Code    26  drv_uart.o(i.UART_SwitchSCLK)
    UART_TransferHandleIRQ                   0x0001107f   Thumb Code   308  drv_uart.o(i.UART_TransferHandleIRQ)
    UART_WriteBlocking                       0x000111b3   Thumb Code    26  drv_uart.o(i.UART_WriteBlocking)
    UART_init                                0x000111cd   Thumb Code   182  drv_uart.o(i.UART_init)
    VIDC_IRQn_Handler                        0x00011289   Thumb Code    18  irq_redirect .o(i.VIDC_IRQn_Handler)
    VPRE_IRQn_Handler                        0x000112a1   Thumb Code    18  irq_redirect .o(i.VPRE_IRQn_Handler)
    WDG_IRQn_Handler                         0x000112b9   Thumb Code    18  irq_redirect .o(i.WDG_IRQn_Handler)
    __0printf                                0x000112d1   Thumb Code    24  printfa.o(i.__0printf)
    __1printf                                0x000112d1   Thumb Code     0  printfa.o(i.__0printf)
    __2printf                                0x000112d1   Thumb Code     0  printfa.o(i.__0printf)
    __c89printf                              0x000112d1   Thumb Code     0  printfa.o(i.__0printf)
    printf                                   0x000112d1   Thumb Code     0  printfa.o(i.__0printf)
    __0vsprintf                              0x000112f1   Thumb Code    30  printfa.o(i.__0vsprintf)
    __1vsprintf                              0x000112f1   Thumb Code     0  printfa.o(i.__0vsprintf)
    __2vsprintf                              0x000112f1   Thumb Code     0  printfa.o(i.__0vsprintf)
    __c89vsprintf                            0x000112f1   Thumb Code     0  printfa.o(i.__0vsprintf)
    vsprintf                                 0x000112f1   Thumb Code     0  printfa.o(i.__0vsprintf)
    __ARM_clz                                0x00011315   Thumb Code    46  depilogue.o(i.__ARM_clz)
    __ARM_common_switch8                     0x00011343   Thumb Code    26  hal_dsi_rx_ctrl.o(i.__ARM_common_switch8)
    __scatterload_copy                       0x0001143d   Thumb Code    14  handlers.o(i.__scatterload_copy)
    __scatterload_zeroinit                   0x0001144b   Thumb Code    14  handlers.o(i.__scatterload_zeroinit)
    __set_errno                              0x00011459   Thumb Code     6  errno.o(i.__set_errno)
    ap_demo                                  0x000121bd   Thumb Code   414  ap_demo.o(i.ap_demo)
    ap_get_tp_calibration_status_01          0x0001259d   Thumb Code    52  app_tp_st_touch.o(i.ap_get_tp_calibration_status_01)
    ap_set_tp_calibration_04                 0x00012791   Thumb Code   186  app_tp_st_touch.o(i.ap_set_tp_calibration_04)
    ap_tp_st_touch_calibration               0x0001285d   Thumb Code   172  app_tp_st_touch.o(i.ap_tp_st_touch_calibration)
    ap_tp_st_touch_error_handler_F3          0x00012925   Thumb Code    16  app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_F3)
    ap_tp_st_touch_error_handler_FF          0x00012935   Thumb Code    34  app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_FF)
    ap_tp_st_touch_get_calibration_success_mark 0x00012959   Thumb Code   164  app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark)
    ap_tp_st_touch_hardware_reset            0x00012a0d   Thumb Code   148  app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset)
    ap_tp_st_touch_scan_point_init           0x00012ae1   Thumb Code    32  app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init)
    ap_tp_st_touch_scan_point_record_event   0x00012b05   Thumb Code   192  app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event)
    ap_tp_st_touch_scan_point_record_event_exec 0x00012bc9   Thumb Code    66  app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec)
    ap_tp_st_touch_simulate_finger_release_event 0x00012c29   Thumb Code    50  app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event)
    app_ADC_IRQn_Handler                     0x00012c65   Thumb Code    22  drv_rxbr.o(i.app_ADC_IRQn_Handler)
    app_AP_NRESET_IRQn_Handler               0x00012c81   Thumb Code    32  drv_gpio.o(i.app_AP_NRESET_IRQn_Handler)
    app_EXTI_INT0_IRQn_Handler               0x00012ca5   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler)
    app_EXTI_INT1_IRQn_Handler               0x00012cc1   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler)
    app_EXTI_INT2_IRQn_Handler               0x00012cdd   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler)
    app_EXTI_INT3_IRQn_Handler               0x00012cf9   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler)
    app_EXTI_INT4_IRQn_Handler               0x00012d15   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler)
    app_EXTI_INT5_IRQn_Handler               0x00012d31   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler)
    app_EXTI_INT6_IRQn_Handler               0x00012d4d   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler)
    app_EXTI_INT7_IRQn_Handler               0x00012d69   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler)
    app_HardFault_Handler                    0x00012d85   Thumb Code    12  drv_common.o(i.app_HardFault_Handler)
    app_I2C0_IRQn_Handler                    0x00012dcd   Thumb Code    14  drv_i2c_slave.o(i.app_I2C0_IRQn_Handler)
    app_I2C1_IRQn_Handler                    0x00012de5   Thumb Code     8  drv_i2c_master.o(i.app_I2C1_IRQn_Handler)
    app_LCDC_IRQn_Handler                    0x00012df5   Thumb Code   146  hal_internal_vsync.o(i.app_LCDC_IRQn_Handler)
    app_MEMC_IRQn_Handler                    0x00012f25   Thumb Code   132  drv_memc.o(i.app_MEMC_IRQn_Handler)
    app_MIPI_RX_IRQn_Handler                 0x00012fad   Thumb Code   232  drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler)
    app_MIPI_TX_IRQn_Handler                 0x00013245   Thumb Code    56  drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler)
    app_PWMDET_IRQn_Handler                  0x000132e5   Thumb Code    62  drv_pwm.o(i.app_PWMDET_IRQn_Handler)
    app_SPIM_IRQn_Handler                    0x0001332d   Thumb Code    34  drv_spi_master.o(i.app_SPIM_IRQn_Handler)
    app_SPIS_IRQn_Handler                    0x0001335d   Thumb Code   500  hal_spi_slave.o(i.app_SPIS_IRQn_Handler)
    app_SWIRE_IRQn_Handler                   0x0001355d   Thumb Code    28  drv_swire.o(i.app_SWIRE_IRQn_Handler)
    app_SysTick_Handler                      0x0001357d   Thumb Code    20  drv_common.o(i.app_SysTick_Handler)
    app_TIMER0_IRQn_Handler                  0x00013595   Thumb Code    10  drv_timer.o(i.app_TIMER0_IRQn_Handler)
    app_TIMER1_IRQn_Handler                  0x0001359f   Thumb Code    10  drv_timer.o(i.app_TIMER1_IRQn_Handler)
    app_TIMER2_IRQn_Handler                  0x000135a9   Thumb Code    10  drv_timer.o(i.app_TIMER2_IRQn_Handler)
    app_TIMER3_IRQn_Handler                  0x000135b3   Thumb Code    10  drv_timer.o(i.app_TIMER3_IRQn_Handler)
    app_UART_IRQn_Handler                    0x000135bd   Thumb Code     8  drv_uart.o(i.app_UART_IRQn_Handler)
    app_VIDC_IRQn_Handler                    0x000135c5   Thumb Code    22  drv_vidc.o(i.app_VIDC_IRQn_Handler)
    app_VPRE_IRQn_Handler                    0x000135e1   Thumb Code    22  drv_rxbr.o(i.app_VPRE_IRQn_Handler)
    app_WDG_IRQn_Handler                     0x000135fd   Thumb Code    52  drv_wdg.o(i.app_WDG_IRQn_Handler)
    app_dma_irq_handler                      0x00013635   Thumb Code    10  drv_dma.o(i.app_dma_irq_handler)
    app_fls_ctrl_Handler                     0x00013645   Thumb Code    38  norflash.o(i.app_fls_ctrl_Handler)
    app_tp_calibration_exec                  0x00013675   Thumb Code    92  app_tp_st_touch.o(i.app_tp_calibration_exec)
    app_tp_init                              0x0001373d   Thumb Code   100  app_tp_transfer.o(i.app_tp_init)
    app_tp_m_read                            0x000137b9   Thumb Code    48  app_tp_transfer.o(i.app_tp_m_read)
    app_tp_m_transfer_complate               0x000137e9   Thumb Code     8  app_tp_transfer.o(i.app_tp_m_transfer_complate)
    app_tp_m_write                           0x000137f1   Thumb Code    16  app_tp_transfer.o(i.app_tp_m_write)
    app_tp_phone_analysis_data               0x00013801   Thumb Code   612  app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data)
    app_tp_phone_clear_reset_on              0x00013ac1   Thumb Code     8  app_tp_transfer.o(i.app_tp_phone_clear_reset_on)
    app_tp_s_read                            0x00013acd   Thumb Code    16  app_tp_transfer.o(i.app_tp_s_read)
    app_tp_s_write                           0x00013add   Thumb Code    16  app_tp_transfer.o(i.app_tp_s_write)
    app_tp_screen_analysis_int               0x00013aed   Thumb Code   588  app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int)
    app_tp_screen_init                       0x00013d6d   Thumb Code    46  app_tp_transfer.o(i.app_tp_screen_init)
    app_tp_transfer_screen_int               0x00013f5d   Thumb Code   330  app_tp_transfer.o(i.app_tp_transfer_screen_int)
    app_tp_transfer_screen_start             0x000140d1   Thumb Code     8  app_tp_transfer.o(i.app_tp_transfer_screen_start)
    blue_change_ccm                          0x000140dd   Thumb Code    58  ap_demo.o(i.blue_change_ccm)
    board_Init                               0x00014119   Thumb Code    30  board.o(i.board_Init)
    calc_framebuffer_setting                 0x0001413d   Thumb Code  1416  hal_internal_vsync.o(i.calc_framebuffer_setting)
    ceil                                     0x000146c9   Thumb Code   180  ceil.o(i.ceil)
    dcs_packet_fifo_alloc                    0x00014841   Thumb Code    80  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    dcs_packet_fifo_init                     0x00014899   Thumb Code    18  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    dcs_packet_free_fifo_header              0x000148b1   Thumb Code    60  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    dcs_packet_get_fifo_header               0x000148f5   Thumb Code    26  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    delayMs                                  0x00014945   Thumb Code    24  tau_delay.o(i.delayMs)
    delayUs                                  0x0001495d   Thumb Code    34  tau_delay.o(i.delayUs)
    drv_ap_rst_trig_edge_detect              0x00014981   Thumb Code    46  drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect)
    drv_chip_info_get_info                   0x000149b9   Thumb Code     6  drv_chip_info.o(i.drv_chip_info_get_info)
    drv_chip_info_init                       0x000149c5   Thumb Code    56  drv_chip_info.o(i.drv_chip_info_init)
    drv_chip_rx_info_check                   0x00014a05   Thumb Code    98  drv_chip_info.o(i.drv_chip_rx_info_check)
    drv_chip_rx_init_done                    0x00014ab5   Thumb Code    16  drv_chip_info.o(i.drv_chip_rx_init_done)
    drv_common_enable_systick                0x00014ac9   Thumb Code    70  drv_common.o(i.drv_common_enable_systick)
    drv_common_system_init                   0x00014b21   Thumb Code     8  drv_common.o(i.drv_common_system_init)
    drv_crgu_config_reset_modules            0x00014b29   Thumb Code    10  drv_crgu.o(i.drv_crgu_config_reset_modules)
    drv_crgu_set_ahb_pre_div                 0x00014b39   Thumb Code    14  drv_crgu.o(i.drv_crgu_set_ahb_pre_div)
    drv_crgu_set_ahb_src                     0x00014b4d   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_ahb_src)
    drv_crgu_set_clock                       0x00014b61   Thumb Code    26  drv_crgu.o(i.drv_crgu_set_clock)
    drv_crgu_set_dpi_mux_src                 0x00014b81   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dpi_mux_src)
    drv_crgu_set_dpi_pre_div                 0x00014b95   Thumb Code    18  drv_crgu.o(i.drv_crgu_set_dpi_pre_div)
    drv_crgu_set_dpi_pre_src                 0x00014bad   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dpi_pre_src)
    drv_crgu_set_dsc_core_div                0x00014bc1   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dsc_core_div)
    drv_crgu_set_dsco_src                    0x00014bd5   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dsco_src)
    drv_crgu_set_dsco_src_div                0x00014be9   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dsco_src_div)
    drv_crgu_set_fb_div                      0x00014bfd   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_fb_div)
    drv_crgu_set_fb_src                      0x00014c11   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_fb_src)
    drv_crgu_set_lcdc_div                    0x00014c25   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_lcdc_div)
    drv_crgu_set_lcdc_src                    0x00014c39   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_lcdc_src)
    drv_crgu_set_mipi_cfg_src                0x00014c4d   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_mipi_cfg_src)
    drv_crgu_set_mipi_ref_src                0x00014c61   Thumb Code    18  drv_crgu.o(i.drv_crgu_set_mipi_ref_src)
    drv_crgu_set_reset                       0x00014c79   Thumb Code    20  drv_crgu.o(i.drv_crgu_set_reset)
    drv_crgu_set_rxbr_div                    0x00014c91   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_rxbr_div)
    drv_crgu_set_rxbr_src                    0x00014ca5   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_rxbr_src)
    drv_crgu_set_vidc_src                    0x00014cb9   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_vidc_src)
    drv_dma_clear_flag                       0x00014ccd   Thumb Code    24  drv_dma.o(i.drv_dma_clear_flag)
    drv_dma_create_handle                    0x00014ce5   Thumb Code    22  drv_dma.o(i.drv_dma_create_handle)
    drv_dma_disenable_channel                0x00014d01   Thumb Code    16  drv_dma.o(i.drv_dma_disenable_channel)
    drv_dma_enable_channel                   0x00014d11   Thumb Code    16  drv_dma.o(i.drv_dma_enable_channel)
    drv_dma_enable_channel_interrupts        0x00014d21   Thumb Code    32  drv_dma.o(i.drv_dma_enable_channel_interrupts)
    drv_dma_get_channel_flag                 0x00014d45   Thumb Code    12  drv_dma.o(i.drv_dma_get_channel_flag)
    drv_dma_irq_handler                      0x00014d51   Thumb Code   138  drv_dma.o(i.drv_dma_irq_handler)
    drv_dma_prepar_transfer                  0x00014de1   Thumb Code    18  drv_dma.o(i.drv_dma_prepar_transfer)
    drv_dma_set_burst                        0x00014df3   Thumb Code    26  drv_dma.o(i.drv_dma_set_burst)
    drv_dma_set_callback                     0x00014e0d   Thumb Code     6  drv_dma.o(i.drv_dma_set_callback)
    drv_dma_set_transfer                     0x00014e15   Thumb Code    62  drv_dma.o(i.drv_dma_set_transfer)
    drv_dsc_dec_convert_pps_rc_parameter     0x00014e59   Thumb Code    54  drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter)
    drv_dsc_dec_disable                      0x00014e8f   Thumb Code    12  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    drv_dsc_dec_enable                       0x00014e9d   Thumb Code    88  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    drv_dsc_dec_get_nslc                     0x00014f11   Thumb Code    10  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    drv_dsc_dec_set_u8_pps                   0x00014f1b   Thumb Code    40  drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps)
    drv_dsi_rx_calc_ipi_tx_delay             0x00014f45   Thumb Code   244  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    drv_dsi_rx_enable_irq                    0x00015049   Thumb Code    58  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    drv_dsi_rx_get_bta_status                0x00015089   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_get_bta_status)
    drv_dsi_rx_get_compression_en            0x00015105   Thumb Code     8  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    drv_dsi_rx_get_max_ret_size              0x0001510d   Thumb Code     6  drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size)
    drv_dsi_rx_power_up                      0x00015113   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    drv_dsi_rx_set_ctrl_cfg                  0x00015121   Thumb Code    32  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    drv_dsi_rx_set_ddi_cfg                   0x00015141   Thumb Code    16  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    drv_dsi_rx_set_ipi_cfg                   0x00015151   Thumb Code    16  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    drv_dsi_rx_set_lane_swap                 0x00015161   Thumb Code    70  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    drv_dsi_rx_set_resp_cnt                  0x000151a7   Thumb Code    38  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    drv_dsi_rx_set_up_phy                    0x000151cd   Thumb Code   256  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    drv_dsi_rx_shut_down                     0x000152d1   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    drv_dsi_tx_command_header                0x000152df   Thumb Code    20  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    drv_dsi_tx_command_mode_cfg              0x000152f3   Thumb Code   108  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    drv_dsi_tx_command_put_payload           0x0001535f   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    drv_dsi_tx_config_eotp                   0x00015363   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    drv_dsi_tx_config_int                    0x0001537b   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    drv_dsi_tx_dpi_lpcmd_time                0x00015383   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    drv_dsi_tx_dpi_mode                      0x0001538b   Thumb Code    10  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    drv_dsi_tx_dpi_polarity                  0x00015395   Thumb Code    36  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    drv_dsi_tx_edpi_cmd_size                 0x000153b9   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    drv_dsi_tx_get_cmd_status                0x000153bd   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    drv_dsi_tx_mode                          0x000153c1   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    drv_dsi_tx_phy_clock_lane_auto_lp        0x000153c5   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    drv_dsi_tx_phy_clock_lane_req_hs         0x000153dd   Thumb Code    26  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    drv_dsi_tx_phy_lane_mode                 0x000153f7   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    drv_dsi_tx_phy_status_ready              0x00015403   Thumb Code   100  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    drv_dsi_tx_phy_status_stopstate          0x00015467   Thumb Code    62  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    drv_dsi_tx_phy_test_setup                0x000154a5   Thumb Code   308  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    drv_dsi_tx_phy_time_cfg                  0x000155d9   Thumb Code    30  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    drv_dsi_tx_powerup                       0x000155f7   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    drv_dsi_tx_response_mode                 0x000155ff   Thumb Code    28  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    drv_dsi_tx_set_bta_ack                   0x0001561b   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    drv_dsi_tx_set_esc_div                   0x00015633   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    drv_dsi_tx_set_int                       0x00015641   Thumb Code    58  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    drv_dsi_tx_set_time_out_div              0x00015681   Thumb Code    16  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    drv_dsi_tx_set_video_chunk               0x00015691   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    drv_dsi_tx_set_video_timing              0x00015699   Thumb Code    34  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    drv_dsi_tx_shutdown                      0x000156bb   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    drv_dsi_tx_timeout_cfg                   0x000156c3   Thumb Code    38  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    drv_dsi_tx_video_mode_cfg                0x000156e9   Thumb Code   170  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    drv_dsi_tx_video_mode_disable_hact_cmd   0x00015793   Thumb Code    22  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_disable_hact_cmd)
    drv_dsi_tx_video_mode_set_lp_cmd         0x000157a9   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd)
    drv_efuse_enter_inactive                 0x000157c1   Thumb Code    46  drv_efuse.o(i.drv_efuse_enter_inactive)
    drv_efuse_int_enable                     0x000157ef   Thumb Code    12  drv_efuse.o(i.drv_efuse_int_enable)
    drv_efuse_read                           0x000157fb   Thumb Code    50  drv_efuse.o(i.drv_efuse_read)
    drv_efuse_read_req                       0x0001582d   Thumb Code    24  drv_efuse.o(i.drv_efuse_read_req)
    drv_gpio_get_input_data                  0x00015845   Thumb Code    20  drv_gpio.o(i.drv_gpio_get_input_data)
    drv_gpio_register_ap_reset_callback      0x0001585d   Thumb Code     6  drv_gpio.o(i.drv_gpio_register_ap_reset_callback)
    drv_gpio_register_callback               0x00015869   Thumb Code    14  drv_gpio.o(i.drv_gpio_register_callback)
    drv_gpio_set_int                         0x0001587d   Thumb Code    74  drv_gpio.o(i.drv_gpio_set_int)
    drv_gpio_set_ioe                         0x000158cd   Thumb Code    26  drv_gpio.o(i.drv_gpio_set_ioe)
    drv_gpio_set_mode0                       0x000158ed   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode0)
    drv_gpio_set_mode1                       0x000158fd   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode1)
    drv_gpio_set_mode2                       0x0001590d   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode2)
    drv_gpio_set_mode3                       0x0001591d   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode3)
    drv_gpio_set_pull_state                  0x0001594d   Thumb Code   298  drv_gpio.o(i.drv_gpio_set_pull_state)
    drv_i2c0_set_callback                    0x00015a7d   Thumb Code     6  drv_i2c_slave.o(i.drv_i2c0_set_callback)
    drv_i2c1_set_callback                    0x00015a89   Thumb Code     6  drv_i2c_master.o(i.drv_i2c1_set_callback)
    drv_i2c_dma_init                         0x00015ac9   Thumb Code   146  drv_i2c_dma.o(i.drv_i2c_dma_init)
    drv_i2c_enable_rx_dma                    0x00015b75   Thumb Code    26  drv_i2c_dma.o(i.drv_i2c_enable_rx_dma)
    drv_i2c_enable_tx_dma                    0x00015b8f   Thumb Code    24  drv_i2c_dma.o(i.drv_i2c_enable_tx_dma)
    drv_i2c_m_clear_it_pending_bit           0x00015ba9   Thumb Code    86  drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit)
    drv_i2c_m_enable                         0x00015c09   Thumb Code    10  drv_i2c_master.o(i.drv_i2c_m_enable)
    drv_i2c_m_enable_intr                    0x00015c19   Thumb Code    42  drv_i2c_master.o(i.drv_i2c_m_enable_intr)
    drv_i2c_master_init                      0x00015c51   Thumb Code   118  drv_i2c_master.o(i.drv_i2c_master_init)
    drv_i2c_master_read_dma                  0x00015cdd   Thumb Code    82  drv_i2c_dma.o(i.drv_i2c_master_read_dma)
    drv_i2c_master_write_dma                 0x00015d39   Thumb Code    50  drv_i2c_dma.o(i.drv_i2c_master_write_dma)
    drv_i2c_s_clear_it_pending_bit           0x00015db3   Thumb Code    66  drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit)
    drv_i2c_s_config_intr                    0x00015df5   Thumb Code     4  drv_i2c_slave.o(i.drv_i2c_s_config_intr)
    drv_i2c_s_enable                         0x00015df9   Thumb Code     8  drv_i2c_slave.o(i.drv_i2c_s_enable)
    drv_i2c_s_get_fifo_status                0x00015e01   Thumb Code    20  drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status)
    drv_i2c_s_set_intr                       0x00015e15   Thumb Code    74  drv_i2c_slave.o(i.drv_i2c_s_set_intr)
    drv_i2c_s_write_data                     0x00015e65   Thumb Code    28  drv_i2c_slave.o(i.drv_i2c_s_write_data)
    drv_i2c_set_dma_irq_callback             0x00015e81   Thumb Code    68  drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback)
    drv_i2c_slave_init                       0x00015ed9   Thumb Code    50  drv_i2c_slave.o(i.drv_i2c_slave_init)
    drv_i2c_slave_write_dma                  0x00015f0d   Thumb Code    20  drv_i2c_dma.o(i.drv_i2c_slave_write_dma)
    drv_lcdc_config_bypass                   0x00015f25   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_config_bypass)
    drv_lcdc_config_ccm                      0x00015f3d   Thumb Code    48  drv_lcdc.o(i.drv_lcdc_config_ccm)
    drv_lcdc_config_disp_mode                0x00015f6d   Thumb Code    22  drv_lcdc.o(i.drv_lcdc_config_disp_mode)
    drv_lcdc_config_dpi_polarity             0x00015f83   Thumb Code    36  drv_lcdc.o(i.drv_lcdc_config_dpi_polarity)
    drv_lcdc_config_dpi_timing               0x00015fa7   Thumb Code    38  drv_lcdc.o(i.drv_lcdc_config_dpi_timing)
    drv_lcdc_config_edpi_mode                0x00015fcd   Thumb Code    22  drv_lcdc.o(i.drv_lcdc_config_edpi_mode)
    drv_lcdc_config_endianness               0x00015fe3   Thumb Code    22  drv_lcdc.o(i.drv_lcdc_config_endianness)
    drv_lcdc_config_input_size               0x00015ff9   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_config_input_size)
    drv_lcdc_config_int                      0x00016005   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_config_int)
    drv_lcdc_config_int_single               0x00016023   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_int_single)
    drv_lcdc_config_overwrite                0x00016045   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_overwrite)
    drv_lcdc_config_overwrite_rgb            0x00016067   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    drv_lcdc_config_partial_display_area     0x00016073   Thumb Code    26  drv_lcdc.o(i.drv_lcdc_config_partial_display_area)
    drv_lcdc_config_partial_display_enable   0x0001608d   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_partial_display_enable)
    drv_lcdc_config_scale_up_coef            0x000160af   Thumb Code    26  drv_lcdc.o(i.drv_lcdc_config_scale_up_coef)
    drv_lcdc_config_scale_up_step            0x000160c9   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_config_scale_up_step)
    drv_lcdc_config_src_parameter            0x000160d5   Thumb Code    76  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    drv_lcdc_config_thresh                   0x00016121   Thumb Code     6  drv_lcdc.o(i.drv_lcdc_config_thresh)
    drv_lcdc_ctrl_flow                       0x00016127   Thumb Code    18  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    drv_lcdc_enable_shadow_reg               0x00016139   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    drv_lcdc_set_int                         0x00016159   Thumb Code    58  drv_lcdc.o(i.drv_lcdc_set_int)
    drv_lcdc_set_prefetch                    0x00016199   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_set_prefetch)
    drv_lcdc_set_video_hw_mode               0x000161b1   Thumb Code    20  drv_lcdc.o(i.drv_lcdc_set_video_hw_mode)
    drv_lcdc_start                           0x000161c5   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_start)
    drv_memc_clear_status                    0x000161e5   Thumb Code    12  drv_memc.o(i.drv_memc_clear_status)
    drv_memc_enable_irq                      0x000161f1   Thumb Code    58  drv_memc.o(i.drv_memc_enable_irq)
    drv_memc_gen_a_tear_signal               0x00016231   Thumb Code    12  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    drv_memc_get_status                      0x0001623d   Thumb Code    18  drv_memc.o(i.drv_memc_get_status)
    drv_memc_rate_transfer_sel               0x0001624f   Thumb Code    16  drv_memc.o(i.drv_memc_rate_transfer_sel)
    drv_memc_sel_vsync                       0x0001625f   Thumb Code    14  drv_memc.o(i.drv_memc_sel_vsync)
    drv_memc_set_active_height               0x0001626d   Thumb Code    14  drv_memc.o(i.drv_memc_set_active_height)
    drv_memc_set_data_mode                   0x00016281   Thumb Code    12  drv_memc.o(i.drv_memc_set_data_mode)
    drv_memc_set_double_buffer               0x0001628d   Thumb Code    16  drv_memc.o(i.drv_memc_set_double_buffer)
    drv_memc_set_double_buffer_reverse       0x0001629d   Thumb Code    18  drv_memc.o(i.drv_memc_set_double_buffer_reverse)
    drv_memc_set_fs_en_conditions            0x000162af   Thumb Code    16  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    drv_memc_set_inten                       0x000162bf   Thumb Code    20  drv_memc.o(i.drv_memc_set_inten)
    drv_memc_set_lcdc_st_conditions          0x000162d5   Thumb Code    18  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    drv_memc_set_ltpo_mode                   0x000162ed   Thumb Code    26  drv_memc.o(i.drv_memc_set_ltpo_mode)
    drv_memc_set_tear_mode                   0x00016307   Thumb Code    14  drv_memc.o(i.drv_memc_set_tear_mode)
    drv_memc_set_tear_waveform               0x00016315   Thumb Code    34  drv_memc.o(i.drv_memc_set_tear_waveform)
    drv_memc_set_vidc_sync_cnt               0x0001633d   Thumb Code    14  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    drv_param_init_get_ccm                   0x0001634d   Thumb Code     4  drv_param_init.o(i.drv_param_init_get_ccm)
    drv_param_init_get_scld_filter_h         0x00016355   Thumb Code    12  drv_param_init.o(i.drv_param_init_get_scld_filter_h)
    drv_param_init_get_scld_filter_v         0x00016369   Thumb Code    12  drv_param_init.o(i.drv_param_init_get_scld_filter_v)
    drv_param_init_get_sclu_filter           0x0001637d   Thumb Code     4  drv_param_init.o(i.drv_param_init_get_sclu_filter)
    drv_param_init_set_ccm                   0x00016385   Thumb Code    14  drv_param_init.o(i.drv_param_init_set_ccm)
    drv_param_init_set_scld_filter           0x00016399   Thumb Code    92  drv_param_init.o(i.drv_param_init_set_scld_filter)
    drv_param_p2r_filter_init                0x000163fd   Thumb Code    30  drv_param_init.o(i.drv_param_p2r_filter_init)
    drv_phy_enable_calibration               0x00016421   Thumb Code    12  drv_phy_common.o(i.drv_phy_enable_calibration)
    drv_phy_get_calibration                  0x00016431   Thumb Code    50  drv_phy_common.o(i.drv_phy_get_calibration)
    drv_phy_get_pll_para                     0x0001646d   Thumb Code    88  drv_phy_common.o(i.drv_phy_get_pll_para)
    drv_phy_get_rate_para                    0x000164cd   Thumb Code    76  drv_phy_common.o(i.drv_phy_get_rate_para)
    drv_phy_test_clear                       0x00016521   Thumb Code    16  drv_phy_common.o(i.drv_phy_test_clear)
    drv_phy_test_lock                        0x00016531   Thumb Code    24  drv_phy_common.o(i.drv_phy_test_lock)
    drv_phy_test_write_1_byte                0x00016549   Thumb Code    32  drv_phy_common.o(i.drv_phy_test_write_1_byte)
    drv_phy_test_write_2_byte                0x00016569   Thumb Code    38  drv_phy_common.o(i.drv_phy_test_write_2_byte)
    drv_phy_test_write_code                  0x0001658f   Thumb Code    30  drv_phy_common.o(i.drv_phy_test_write_code)
    drv_pwr_set_cp_mode                      0x000165cd   Thumb Code    26  drv_pwr.o(i.drv_pwr_set_cp_mode)
    drv_pwr_set_pvd_mode                     0x000165ed   Thumb Code    18  drv_pwr.o(i.drv_pwr_set_pvd_mode)
    drv_pwr_set_system_clk_src               0x00016605   Thumb Code    44  drv_pwr.o(i.drv_pwr_set_system_clk_src)
    drv_rxbr_clear_pkt_buffer                0x00016683   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    drv_rxbr_clear_status0                   0x0001668d   Thumb Code     4  drv_rxbr.o(i.drv_rxbr_clear_status0)
    drv_rxbr_enable_irq                      0x00016691   Thumb Code    90  drv_rxbr.o(i.drv_rxbr_enable_irq)
    drv_rxbr_frame_drop_cfg                  0x000166ed   Thumb Code    16  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    drv_rxbr_get_clk                         0x00016701   Thumb Code    66  drv_rxbr.o(i.drv_rxbr_get_clk)
    drv_rxbr_get_col_addr                    0x00016765   Thumb Code     4  drv_rxbr.o(i.drv_rxbr_get_col_addr)
    drv_rxbr_get_page_addr                   0x0001677b   Thumb Code     4  drv_rxbr.o(i.drv_rxbr_get_page_addr)
    drv_rxbr_get_pkt_buf_error_status        0x0001677f   Thumb Code    12  drv_rxbr.o(i.drv_rxbr_get_pkt_buf_error_status)
    drv_rxbr_hline_rcv1_cfg                  0x000167b3   Thumb Code    12  drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg)
    drv_rxbr_hline_rcv_cfg                   0x000167bf   Thumb Code     8  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    drv_rxbr_register_irq0_callback          0x000167c9   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_register_irq0_callback)
    drv_rxbr_register_irq1_callback          0x000167d5   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    drv_rxbr_set_ack_pkt_header              0x000167e1   Thumb Code    20  drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header)
    drv_rxbr_set_color_format                0x000167f5   Thumb Code    20  drv_rxbr.o(i.drv_rxbr_set_color_format)
    drv_rxbr_set_filter_regs                 0x00016809   Thumb Code    18  drv_rxbr.o(i.drv_rxbr_set_filter_regs)
    drv_rxbr_set_inten                       0x0001681b   Thumb Code    20  drv_rxbr.o(i.drv_rxbr_set_inten)
    drv_rxbr_set_ltpo_drop_th                0x0001682f   Thumb Code    16  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    drv_rxbr_set_usr_cfg                     0x0001683f   Thumb Code    38  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    drv_rxbr_set_usr_col                     0x00016865   Thumb Code     8  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    drv_rxbr_set_usr_row                     0x0001686d   Thumb Code     8  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    drv_spi_m_read_data                      0x00016875   Thumb Code    28  drv_spi_master.o(i.drv_spi_m_read_data)
    drv_swire_enable                         0x00016895   Thumb Code    24  drv_swire.o(i.drv_swire_enable)
    drv_swire_set_int                        0x000168b1   Thumb Code    76  drv_swire.o(i.drv_swire_set_int)
    drv_swire_set_power_down                 0x00016905   Thumb Code    24  drv_swire.o(i.drv_swire_set_power_down)
    drv_sys_cfg_clear_all_int                0x00016921   Thumb Code     8  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    drv_sys_cfg_clear_pending                0x0001692d   Thumb Code    32  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    drv_sys_cfg_sel_ap_rst_lvl_trig          0x00016955   Thumb Code    18  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig)
    drv_sys_cfg_sel_ap_rst_trig              0x0001696d   Thumb Code    22  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig)
    drv_sys_cfg_sel_gpio_group               0x00016989   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group)
    drv_sys_cfg_sel_int_trig                 0x000169ad   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig)
    drv_sys_cfg_set_dma_rx_req               0x000169d1   Thumb Code    10  drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req)
    drv_sys_cfg_set_dma_tx_req               0x000169e1   Thumb Code    10  drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req)
    drv_sys_cfg_set_int                      0x000169f1   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    drv_timer_enable                         0x00016a2f   Thumb Code    32  drv_timer.o(i.drv_timer_enable)
    drv_timer_get_instance                   0x00016a51   Thumb Code    10  drv_timer.o(i.drv_timer_get_instance)
    drv_timer_get_prescaler                  0x00016a61   Thumb Code    12  drv_timer.o(i.drv_timer_get_prescaler)
    drv_timer_register_callback              0x00016ab5   Thumb Code    14  drv_timer.o(i.drv_timer_register_callback)
    drv_timer_set_compare_val                0x00016ac9   Thumb Code    16  drv_timer.o(i.drv_timer_set_compare_val)
    drv_timer_set_int                        0x00016ad9   Thumb Code    80  drv_timer.o(i.drv_timer_set_int)
    drv_timer_set_prescaler                  0x00016b2d   Thumb Code    36  drv_timer.o(i.drv_timer_set_prescaler)
    drv_timer_set_repeat                     0x00016b55   Thumb Code    12  drv_timer.o(i.drv_timer_set_repeat)
    drv_tx_phy_test_enter                    0x00016b6f   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    drv_tx_phy_test_exit                     0x00016b8b   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    drv_vidc_clear_irq                       0x00016bdd   Thumb Code     8  drv_vidc.o(i.drv_vidc_clear_irq)
    drv_vidc_enable                          0x00016be5   Thumb Code    24  drv_vidc.o(i.drv_vidc_enable)
    drv_vidc_enable_irq                      0x00016bfd   Thumb Code    58  drv_vidc.o(i.drv_vidc_enable_irq)
    drv_vidc_get_irq_status                  0x00016c3d   Thumb Code    18  drv_vidc.o(i.drv_vidc_get_irq_status)
    drv_vidc_init_module_enable              0x00016c51   Thumb Code    36  drv_vidc.o(i.drv_vidc_init_module_enable)
    drv_vidc_register_callback               0x00016c79   Thumb Code     6  drv_vidc.o(i.drv_vidc_register_callback)
    drv_vidc_reset                           0x00016c85   Thumb Code     6  drv_vidc.o(i.drv_vidc_reset)
    drv_vidc_set_dst_parameter               0x00016c8b   Thumb Code    60  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    drv_vidc_set_irqen                       0x00016cc7   Thumb Code    20  drv_vidc.o(i.drv_vidc_set_irqen)
    drv_vidc_set_mirror                      0x00016cdb   Thumb Code    16  drv_vidc.o(i.drv_vidc_set_mirror)
    drv_vidc_set_p2r_hcoef0                  0x00016ceb   Thumb Code     8  drv_vidc.o(i.drv_vidc_set_p2r_hcoef0)
    drv_vidc_set_p2r_hinitb                  0x00016cf3   Thumb Code    38  drv_vidc.o(i.drv_vidc_set_p2r_hinitb)
    drv_vidc_set_p2r_hinitr                  0x00016d19   Thumb Code    38  drv_vidc.o(i.drv_vidc_set_p2r_hinitr)
    drv_vidc_set_pentile_swap                0x00016d41   Thumb Code    18  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    drv_vidc_set_pu_ctrl                     0x00016d59   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    drv_vidc_set_rotation                    0x00016d63   Thumb Code    16  drv_vidc.o(i.drv_vidc_set_rotation)
    drv_vidc_set_scld_hcoef0                 0x00016d73   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    drv_vidc_set_scld_hcoef1                 0x00016d7d   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    drv_vidc_set_scld_step                   0x00016d87   Thumb Code    18  drv_vidc.o(i.drv_vidc_set_scld_step)
    drv_vidc_set_scld_vcoef0                 0x00016d99   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    drv_vidc_set_scld_vcoef1                 0x00016da3   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    drv_vidc_set_src_parameter               0x00016dad   Thumb Code    22  drv_vidc.o(i.drv_vidc_set_src_parameter)
    drv_wdg_clear_counter                    0x00016dc5   Thumb Code    12  drv_wdg.o(i.drv_wdg_clear_counter)
    drv_wdg_set_int                          0x00016df5   Thumb Code    60  drv_wdg.o(i.drv_wdg_set_int)
    finger_calibration_init                  0x00016e35   Thumb Code    14  ap_demo.o(i.finger_calibration_init)
    fls_clr_interrupt_flag                   0x00016e49   Thumb Code    10  drv_fls.o(i.fls_clr_interrupt_flag)
    fputc                                    0x00016e53   Thumb Code    20  tau_log.o(i.fputc)
    hal_dsi_rx_ctrl_ack_long_cmd             0x00016e69   Thumb Code    84  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd)
    hal_dsi_rx_ctrl_create_handle            0x00016ec1   Thumb Code    48  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    hal_dsi_rx_ctrl_deinit                   0x00016ef5   Thumb Code   158  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit)
    hal_dsi_rx_ctrl_dsc_async_handler        0x00016fa5   Thumb Code    34  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler)
    hal_dsi_rx_ctrl_gen_a_tear_signal        0x00016fcd   Thumb Code    32  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal)
    hal_dsi_rx_ctrl_get_max_ret_size         0x00016ff5   Thumb Code    30  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size)
    hal_dsi_rx_ctrl_init                     0x0001701d   Thumb Code   144  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    hal_dsi_rx_ctrl_pre_init_pps             0x0001780d   Thumb Code    56  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    hal_dsi_rx_ctrl_send_ack_cmd             0x00017849   Thumb Code   212  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd)
    hal_dsi_rx_ctrl_set_cus_scld_filter      0x00017939   Thumb Code    98  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter)
    hal_dsi_rx_ctrl_set_hw_tear_mode         0x000179a5   Thumb Code    42  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode)
    hal_dsi_rx_ctrl_set_sw_tear_mode         0x00017a85   Thumb Code    42  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode)
    hal_dsi_rx_ctrl_set_tear_mode_ex         0x00017ab9   Thumb Code    14  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex)
    hal_dsi_rx_ctrl_start                    0x00017ac9   Thumb Code    46  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    hal_dsi_rx_ctrl_stop                     0x00017b05   Thumb Code    46  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop)
    hal_dsi_rx_ctrl_toggle_resolution        0x00017b41   Thumb Code    28  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    hal_dsi_tx_ctrl_create_handle            0x0001814d   Thumb Code    34  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    hal_dsi_tx_ctrl_deinit                   0x00018179   Thumb Code   118  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit)
    hal_dsi_tx_ctrl_enter_init_panel_mode    0x000181fd   Thumb Code    68  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode)
    hal_dsi_tx_ctrl_exit_init_panel_mode     0x00018249   Thumb Code    32  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode)
    hal_dsi_tx_ctrl_init                     0x00018271   Thumb Code   154  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    hal_dsi_tx_ctrl_panel_reset_pin          0x00018339   Thumb Code    12  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin)
    hal_dsi_tx_ctrl_set_ccm                  0x00018345   Thumb Code    28  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm)
    hal_dsi_tx_ctrl_set_overwrite_rgb        0x00018365   Thumb Code    16  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    hal_dsi_tx_ctrl_set_partial_disp         0x00018379   Thumb Code    12  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp)
    hal_dsi_tx_ctrl_set_partial_disp_area    0x00018389   Thumb Code    30  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area)
    hal_dsi_tx_ctrl_start                    0x000183ad   Thumb Code   150  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    hal_dsi_tx_ctrl_stop                     0x00018455   Thumb Code    56  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop)
    hal_dsi_tx_ctrl_write_cmd                0x00018499   Thumb Code   200  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    hal_gpio_ctrl_eint                       0x00018749   Thumb Code    18  hal_gpio.o(i.hal_gpio_ctrl_eint)
    hal_gpio_get_input_data                  0x00018761   Thumb Code    18  hal_gpio.o(i.hal_gpio_get_input_data)
    hal_gpio_init_eint                       0x00018775   Thumb Code    58  hal_gpio.o(i.hal_gpio_init_eint)
    hal_gpio_init_input                      0x000187b5   Thumb Code    28  hal_gpio.o(i.hal_gpio_init_input)
    hal_gpio_init_output                     0x000187d5   Thumb Code    34  hal_gpio.o(i.hal_gpio_init_output)
    hal_gpio_reg_eint_cb                     0x000187fd   Thumb Code    20  hal_gpio.o(i.hal_gpio_reg_eint_cb)
    hal_gpio_set_ap_reset_int                0x00018815   Thumb Code    76  hal_gpio.o(i.hal_gpio_set_ap_reset_int)
    hal_gpio_set_mode                        0x00018865   Thumb Code    90  hal_gpio.o(i.hal_gpio_set_mode)
    hal_gpio_set_output_data                 0x000188c5   Thumb Code     8  hal_gpio.o(i.hal_gpio_set_output_data)
    hal_gpio_set_pull_state                  0x000188cd   Thumb Code    26  hal_gpio.o(i.hal_gpio_set_pull_state)
    hal_i2c_m_dma_init                       0x000188ed   Thumb Code    92  hal_i2c_master.o(i.hal_i2c_m_dma_init)
    hal_i2c_m_dma_read                       0x00018959   Thumb Code    26  hal_i2c_master.o(i.hal_i2c_m_dma_read)
    hal_i2c_m_dma_write                      0x00018979   Thumb Code    24  hal_i2c_master.o(i.hal_i2c_m_dma_write)
    hal_i2c_m_transfer_complate              0x00018995   Thumb Code     6  hal_i2c_master.o(i.hal_i2c_m_transfer_complate)
    hal_i2c_s_dma_write                      0x000189d1   Thumb Code    62  hal_i2c_slave.o(i.hal_i2c_s_dma_write)
    hal_i2c_s_init                           0x00018a1d   Thumb Code   176  hal_i2c_slave.o(i.hal_i2c_s_init)
    hal_i2c_s_nonblocking_read               0x00018ae5   Thumb Code    14  hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read)
    hal_i2c_s_set_transfer                   0x00018af9   Thumb Code     6  hal_i2c_slave.o(i.hal_i2c_s_set_transfer)
    hal_internal_check_video_auto_sync       0x00018c79   Thumb Code    18  hal_internal_vsync.o(i.hal_internal_check_video_auto_sync)
    hal_internal_init_memc                   0x00018c91   Thumb Code   170  hal_internal_vsync.o(i.hal_internal_init_memc)
    hal_internal_rx_dcs_async_handler        0x00018d8d   Thumb Code    42  hal_internal_vsync.o(i.hal_internal_rx_dcs_async_handler)
    hal_internal_rx_dcs_polling              0x00018db9   Thumb Code    78  hal_internal_vsync.o(i.hal_internal_rx_dcs_polling)
    hal_internal_sync_get_fb_setting         0x00018e11   Thumb Code    12  hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting)
    hal_internal_sync_get_hight_performan_mode 0x00018e21   Thumb Code    10  hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode)
    hal_internal_sync_input_resolution_change 0x00018e31   Thumb Code   438  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    hal_internal_vsync_deinit                0x0001905d   Thumb Code    30  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    hal_internal_vsync_get_rx_state          0x00019085   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state)
    hal_internal_vsync_get_sync_line         0x00019091   Thumb Code    18  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    hal_internal_vsync_get_tear_mode         0x000190a9   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_tear_mode)
    hal_internal_vsync_get_tx_state          0x000190b5   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    hal_internal_vsync_init_rx               0x000190c1   Thumb Code   274  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    hal_internal_vsync_init_tx               0x00019201   Thumb Code   172  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    hal_internal_vsync_set_auto_hw_filter    0x000192b1   Thumb Code   132  hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter)
    hal_internal_vsync_set_rx_state          0x00019341   Thumb Code    30  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    hal_internal_vsync_set_tear_mode         0x00019365   Thumb Code    72  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    hal_internal_vsync_set_tx_state          0x000193b5   Thumb Code   122  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    hal_intl_svs_deinit_tx                   0x00019439   Thumb Code    10  hal_internal_soft_sync.o(i.hal_intl_svs_deinit_tx)
    hal_intl_svs_handle                      0x00019449   Thumb Code    24  hal_internal_soft_sync.o(i.hal_intl_svs_handle)
    hal_intl_svs_init_rx                     0x0001946d   Thumb Code   108  hal_internal_soft_sync.o(i.hal_intl_svs_init_rx)
    hal_intl_svs_init_tx                     0x000194e5   Thumb Code    16  hal_internal_soft_sync.o(i.hal_intl_svs_init_tx)
    hal_intl_svs_update_rxbr_clk             0x000194f9   Thumb Code    52  hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk)
    hal_spi_m_clear_rxfifo                   0x000199a1   Thumb Code    14  hal_spi_master.o(i.hal_spi_m_clear_rxfifo)
    hal_swire_deinit                         0x000199af   Thumb Code    18  hal_swire.o(i.hal_swire_deinit)
    hal_swire_open                           0x000199c1   Thumb Code    22  hal_swire.o(i.hal_swire_open)
    hal_system_enable_systick                0x000199d7   Thumb Code     8  hal_system.o(i.hal_system_enable_systick)
    hal_system_init                          0x000199e1   Thumb Code   104  hal_system.o(i.hal_system_init)
    hal_system_init_console                  0x00019a69   Thumb Code    28  hal_system.o(i.hal_system_init_console)
    hal_system_set_phy_calibration           0x00019a85   Thumb Code     8  hal_system.o(i.hal_system_set_phy_calibration)
    hal_system_set_pvd                       0x00019a8d   Thumb Code     8  hal_system.o(i.hal_system_set_pvd)
    hal_system_set_vcc                       0x00019a95   Thumb Code     8  hal_system.o(i.hal_system_set_vcc)
    hal_timer_deinit                         0x00019a9d   Thumb Code    46  hal_timer.o(i.hal_timer_deinit)
    hal_timer_init                           0x00019acb   Thumb Code    26  hal_timer.o(i.hal_timer_init)
    hal_timer_start                          0x00019ae5   Thumb Code    66  hal_timer.o(i.hal_timer_start)
    hal_timer_stop                           0x00019b2d   Thumb Code    40  hal_timer.o(i.hal_timer_stop)
    hal_uart_init                            0x00019b85   Thumb Code   126  hal_uart.o(i.hal_uart_init)
    hal_uart_transmit_blocking               0x00019c11   Thumb Code    12  hal_uart.o(i.hal_uart_transmit_blocking)
    handle_init                              0x00019c21   Thumb Code   140  irq_redirect .o(i.handle_init)
    main                                     0x0001c83f   Thumb Code    16  main.o(i.main)
    sqrt                                     0x0001d6e1   Thumb Code    66  sqrt.o(i.sqrt)
    tp_heartbeat_exec                        0x0001da6d   Thumb Code    70  ap_demo.o(i.tp_heartbeat_exec)
    wCRCTalbeAbs                             0x0001e084   Data          32  app_tp_st_touch.o(.constdata)
    phone_b6_00_28_data                      0x0001e1bc   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_b6_00_28_back                      0x0001e1c0   Data           8  app_tp_for_custom_s8.o(.constdata)
    phone_b6_00_08_data                      0x0001e1c8   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_b6_00_08_back                      0x0001e1cb   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_b6_00_04_data                      0x0001e1ce   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_b6_00_04_back                      0x0001e1d1   Data           7  app_tp_for_custom_s8.o(.constdata)
    phone_b8_00_08_data                      0x0001e1d8   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_b8_00_08_back                      0x0001e1db   Data           8  app_tp_for_custom_s8.o(.constdata)
    phone_ac_data                            0x0001e1e3   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_ac_back                            0x0001e1e4   Data           8  app_tp_for_custom_s8.o(.constdata)
    phone_a7_data                            0x0001e1ec   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_a7_back                            0x0001e1ed   Data           8  app_tp_for_custom_s8.o(.constdata)
    phone_84_data                            0x0001e1f5   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_84_back                            0x0001e1f6   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_aa_00_data                         0x0001e1fa   Data           2  app_tp_for_custom_s8.o(.constdata)
    phone_aa_00_back                         0x0001e1fc   Data           8  app_tp_for_custom_s8.o(.constdata)
    phone_aa_01_data                         0x0001e204   Data           2  app_tp_for_custom_s8.o(.constdata)
    phone_aa_01_back                         0x0001e206   Data           8  app_tp_for_custom_s8.o(.constdata)
    phone_d0_00_5a_data                      0x0001e20e   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_d0_00_5a_back                      0x0001e211   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_d0_00_5c_data                      0x0001e215   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_d0_00_5c_back                      0x0001e218   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_d0_00_64_data                      0x0001e21c   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_d0_00_64_back                      0x0001e21f   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_d0_00_88_data                      0x0001e222   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_d0_00_88_back                      0x0001e225   Data           5  app_tp_for_custom_s8.o(.constdata)
    phone_d0_00_7a_data                      0x0001e22a   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_d0_00_7a_back                      0x0001e22d   Data          15  app_tp_for_custom_s8.o(.constdata)
    phone_d0_76_04_data                      0x0001e23c   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_d0_76_04_back                      0x0001e23f   Data           5  app_tp_for_custom_s8.o(.constdata)
    phone_d0_00_50_data                      0x0001e244   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_d0_00_50_back                      0x0001e247   Data           8  app_tp_for_custom_s8.o(.constdata)
    phone_d0_1f_6e_data                      0x0001e24f   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_d0_1f_6e_back                      0x0001e252   Data           5  app_tp_for_custom_s8.o(.constdata)
    phone_d0_1f_b3_data                      0x0001e257   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_d0_1f_b3_back                      0x0001e25a   Data           5  app_tp_for_custom_s8.o(.constdata)
    phone_d0_1f_6c_data                      0x0001e25f   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_d0_1f_6c_back                      0x0001e262   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_d0_1f_b2_data                      0x0001e265   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_d0_1f_b2_back                      0x0001e268   Data           2  app_tp_for_custom_s8.o(.constdata)
    phone_d0_1f_72_data                      0x0001e26a   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_d0_1f_72_back                      0x0001e26d   Data          33  app_tp_for_custom_s8.o(.constdata)
    phone_d0_00_06_data                      0x0001e28e   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_d0_00_06_back                      0x0001e291   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_d0_23_ac_data                      0x0001e295   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_d0_23_ac_back                      0x0001e298   Data         129  app_tp_for_custom_s8.o(.constdata)
    phone_d0_24_2c_data                      0x0001e319   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_d0_24_2c_back                      0x0001e31c   Data         129  app_tp_for_custom_s8.o(.constdata)
    phone_d0_24_ac_data                      0x0001e39d   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_d0_24_ac_back                      0x0001e3a0   Data         129  app_tp_for_custom_s8.o(.constdata)
    phone_d0_25_2c_data                      0x0001e421   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_d0_25_2c_back                      0x0001e424   Data         129  app_tp_for_custom_s8.o(.constdata)
    phone_d0_25_ac_data                      0x0001e4a5   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_d0_25_ac_back                      0x0001e4a8   Data         129  app_tp_for_custom_s8.o(.constdata)
    phone_d0_26_2c_data                      0x0001e529   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_d0_26_2c_back                      0x0001e52c   Data         129  app_tp_for_custom_s8.o(.constdata)
    phone_d0_26_ac_data                      0x0001e5ad   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_d0_26_ac_back                      0x0001e5b0   Data         129  app_tp_for_custom_s8.o(.constdata)
    phone_d0_27_2c_data                      0x0001e631   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_d0_27_2c_back                      0x0001e634   Data         129  app_tp_for_custom_s8.o(.constdata)
    phone_data_86_1                          0x0001e6b5   Data           8  app_tp_for_custom_s8.o(.constdata)
    phone_data_86_2                          0x0001e6bd   Data           8  app_tp_for_custom_s8.o(.constdata)
    phone_data_86_3                          0x0001e6c5   Data           8  app_tp_for_custom_s8.o(.constdata)
    phone_data_86_4                          0x0001e6cd   Data           8  app_tp_for_custom_s8.o(.constdata)
    phone_data_A6_1                          0x0001e6d5   Data         208  app_tp_for_custom_s8.o(.constdata)
    phone_data_A6_2                          0x0001e7a5   Data          28  app_tp_for_custom_s8.o(.constdata)
    phone_data_FA                            0x0001e7c1   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_C105                          0x0001e7c2   Data           7  app_tp_for_custom_s8.o(.constdata)
    phone_data_C112_0                        0x0001e7c9   Data           8  app_tp_for_custom_s8.o(.constdata)
    phone_data_C112_22                       0x0001e7d1   Data           8  app_tp_for_custom_s8.o(.constdata)
    phone_data_C112_23                       0x0001e7d9   Data           8  app_tp_for_custom_s8.o(.constdata)
    phone_data_C112_12                       0x0001e7e1   Data           8  app_tp_for_custom_s8.o(.constdata)
    phone_data_C112_13                       0x0001e7e9   Data           8  app_tp_for_custom_s8.o(.constdata)
    phone_data_C112_02                       0x0001e7f1   Data           8  app_tp_for_custom_s8.o(.constdata)
    phone_data_C112_03                       0x0001e7f9   Data           8  app_tp_for_custom_s8.o(.constdata)
    screen_87_data                           0x0001e801   Data           1  app_tp_for_custom_s8.o(.constdata)
    screen_a0_00_ff_data                     0x0001e802   Data           3  app_tp_for_custom_s8.o(.constdata)
    screen_a4_06_c1_data                     0x0001e805   Data           3  app_tp_for_custom_s8.o(.constdata)
    sleep_on                                 0x0001e808   Data           8  app_tp_for_custom_s8.o(.constdata)
    screen_reg_int_data_size                 0x0001e810   Data           1  app_tp_for_custom_s8.o(.constdata)
    screen_reg_start_data_size               0x0001e811   Data           1  app_tp_for_custom_s8.o(.constdata)
    Region$$Table$$Base                      0x0001ebf8   Number         0  anon$$obj.o(Region$$Table)
    Region$$Table$$Limit                     0x0001ec28   Number         0  anon$$obj.o(Region$$Table)
    g_fun_handle                             0x00070100   Data         192  irq_redirect .o(.ARM.__AT_0x00070100)
    phone_DoubleDlick_flag                   0x000701e2   Data           1  ap_demo.o(.data)
    phone_86_flag                            0x000701e3   Data           1  ap_demo.o(.data)
    phone_A6_flag                            0x000701e4   Data           1  ap_demo.o(.data)
    phone_start_flag                         0x000701e5   Data           1  ap_demo.o(.data)
    phone_DisplayOFF_count                   0x000701e6   Data           2  ap_demo.o(.data)
    phone_DisplayOFF_flag                    0x000701e8   Data           1  ap_demo.o(.data)
    s_finger_calibration                     0x000701ea   Data           6  ap_demo.o(.data)
    s_heartbeat                              0x000701f0   Data           4  ap_demo.o(.data)
    value_reg_b1                             0x000703f4   Data           2  ap_demo.o(.data)
    value_reg_ca                             0x000703f6   Data           2  ap_demo.o(.data)
    value_reg_ca_bak                         0x00070404   Data           2  ap_demo.o(.data)
    value_reg_b1_bak                         0x00070406   Data           2  ap_demo.o(.data)
    read_point                               0x00070418   Data           1  app_tp_transfer.o(.data)
    s_screen_number                          0x00070419   Data           2  app_tp_transfer.o(.data)
    s_screen_temp                            0x0007041b   Data           2  app_tp_transfer.o(.data)
    s_screen_read_MI10Pro                    0x0007041d   Data           8  app_tp_transfer.o(.data)
    s_screen_init_complate                   0x00070429   Data           1  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data1               0x0007042b   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data2               0x0007042e   Data           6  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data3               0x00070434   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data4               0x00070437   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data5               0x0007043a   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data6               0x0007043d   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data7               0x00070440   Data           5  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data8               0x00070445   Data           6  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data9               0x0007044b   Data           2  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data10              0x0007044d   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data11              0x00070450   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data12              0x00070453   Data           3  app_tp_transfer.o(.data)
    st_touch_init_sensor_off                 0x0007045a   Data           3  app_tp_st_touch.o(.data)
    st_touch_init_sensor_on                  0x0007045d   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_reset                 0x00070460   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_FpnlInit              0x00070463   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_PnlInit               0x00070466   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_TuneM                 0x00070469   Data           4  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_TuneS                 0x0007046d   Data           4  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_SvCfg                 0x00070471   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_SvCx                  0x00070474   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_SvPnl                 0x00070477   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_clearfifo             0x0007047a   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_clkreset              0x0007047d   Data           3  app_tp_st_touch.o(.data)
    phone_data_B1                            0x000704ac   Data           2  app_tp_for_custom_s8.o(.data)
    tp_flag                                  0x000704ae   Data           1  app_tp_for_custom_s8.o(.data)
    s8_host_num                              0x000704af   Data          11  app_tp_for_custom_s8.o(.data)
    s8_host_id                               0x000704ba   Data          10  app_tp_for_custom_s8.o(.data)
    phone_touch_flag                         0x000704c4   Data           1  app_tp_for_custom_s8.o(.data)
    tp_sleep_in                              0x000704c5   Data           1  app_tp_for_custom_s8.o(.data)
    tp_sleep_count                           0x000704c6   Data           1  app_tp_for_custom_s8.o(.data)
    sleep_double_EN                          0x000704c7   Data           1  app_tp_for_custom_s8.o(.data)
    sleep_double_Click_off                   0x000704c8   Data           1  app_tp_for_custom_s8.o(.data)
    g_screen_input_rst_pad                   0x000704d2   Data           1  app_tp_for_custom_s8.o(.data)
    g_screen_input_int_pad                   0x000704d3   Data           1  app_tp_for_custom_s8.o(.data)
    g_phone_input_rst_pad                    0x000704d4   Data           1  app_tp_for_custom_s8.o(.data)
    g_phone_output_int_pad                   0x000704d5   Data           1  app_tp_for_custom_s8.o(.data)
    phone_86_Count                           0x000704dc   Data           1  app_tp_for_custom_s8.o(.data)
    screen_data_write_1                      0x000704dd   Data           1  app_tp_for_custom_s8.o(.data)
    screen_data_write_2                      0x000704de   Data           3  app_tp_for_custom_s8.o(.data)
    screen_data_write_3                      0x000704e1   Data           5  app_tp_for_custom_s8.o(.data)
    screen_data_write_4                      0x000704e6   Data           2  app_tp_for_custom_s8.o(.data)
    screen_data_write_5                      0x000704e8   Data           2  app_tp_for_custom_s8.o(.data)
    screen_data_write_6                      0x000704ea   Data           2  app_tp_for_custom_s8.o(.data)
    screen_data_write_7                      0x000704ec   Data           2  app_tp_for_custom_s8.o(.data)
    screen_data_write_8                      0x000704ee   Data           2  app_tp_for_custom_s8.o(.data)
    screen_data_write_9                      0x000704f0   Data           2  app_tp_for_custom_s8.o(.data)
    screen_data_write_10                     0x000704f2   Data           2  app_tp_for_custom_s8.o(.data)
    screen_data_write_11                     0x000704f4   Data           1  app_tp_for_custom_s8.o(.data)
    screen_data_write_12                     0x000704f5   Data           1  app_tp_for_custom_s8.o(.data)
    screen_reg_int_data                      0x000704f8   Data          48  app_tp_for_custom_s8.o(.data)
    screen_reg_start_data                    0x00070528   Data          64  app_tp_for_custom_s8.o(.data)
    phone_reg_point_data                     0x00070568   Data           3  app_tp_for_custom_s8.o(.data)
    phone_reg_point_back                     0x0007056b   Data           2  app_tp_for_custom_s8.o(.data)
    phone_reg_coord_data                     0x0007056d   Data           1  app_tp_for_custom_s8.o(.data)
    phone_reg_coord_back                     0x0007056e   Data          80  app_tp_for_custom_s8.o(.data)
    phone_reg_int_data                       0x000705c0   Data          32  app_tp_for_custom_s8.o(.data)
    phone_reg_int_size                       0x000705e0   Data           1  app_tp_for_custom_s8.o(.data)
    phone_reg_const_data                     0x000705e4   Data         480  app_tp_for_custom_s8.o(.data)
    phone_reg_const_data_size                0x000707c4   Data           1  app_tp_for_custom_s8.o(.data)
    g_sof_gen_te_func                        0x000707d0   Data           4  hal_internal_vsync.o(.data)
    g_systick_cb_func                        0x000707e4   Data           4  drv_common.o(.data)
    g_system_clock                           0x000707e8   Data           4  drv_common.o(.data)
    g_scld_fhd_filter_h                      0x00070800   Data         256  drv_param_init.o(.data)
    g_scld_fhd_filter_v                      0x00070900   Data         256  drv_param_init.o(.data)
    g_scld_hd_filter_h                       0x00070a00   Data         256  drv_param_init.o(.data)
    g_scld_hd_filter_v                       0x00070b00   Data         256  drv_param_init.o(.data)
    g_sclu_lanczos_filter                    0x00070c00   Data         128  drv_param_init.o(.data)
    g_ccm_setting                            0x00070c80   Data          36  drv_param_init.o(.data)
    g_int_rxbr_irq0_cb_func                  0x00070d04   Data           4  drv_rxbr.o(.data)
    g_int_rxbr_irq1_cb_func                  0x00070d08   Data           4  drv_rxbr.o(.data)
    g_int_vidc_cb_func                       0x00070d0c   Data           4  drv_vidc.o(.data)
    g_fls_w_cmd                              0x00070d20   Data           1  norflash.o(.data)
    g_fls_r_cmd                              0x00070d21   Data           1  norflash.o(.data)
    g_fls_write_en_status                    0x00070d22   Data           1  norflash.o(.data)
    isFlsTransferEnd                         0x00070d23   Data           1  norflash.o(.data)
    isFlsFifoReq                             0x00070d24   Data           1  norflash.o(.data)
    isNandWriteCompleted                     0x00070d25   Data           1  norflash.o(.data)
    isNandReadCompleted                      0x00070d26   Data           1  norflash.o(.data)
    g_fls_error_info                         0x00070d2c   Data           6  norflash.o(.data)
    __stdout                                 0x00070d54   Data           4  stdout.o(.data)
    s_screen_read_bak                        0x00070d5c   Data          80  app_tp_transfer.o(.bss)
    s_screen_read_MI10Pro_1                  0x00070f3c   Data         100  app_tp_transfer.o(.bss)
    tp_scan_data                             0x00070fa0   Data          12  app_tp_st_touch.o(.bss)
    string                                   0x000710bc   Data         256  tau_log.o(.bss)
    hal_dmahandle                            0x000711bc   Data         160  hal_uart.o(.bss)
    hal_uarthandle_dma                       0x0007125c   Data          32  hal_uart.o(.bss)
    hal_uart_handle_global                   0x0007127c   Data          16  hal_uart.o(.bss)
    g_vsync_hande                            0x0007128c   Data          84  hal_internal_vsync.o(.bss)
    g_dcs_execute_table                      0x000712e0   Data        2048  hal_internal_vsync.o(.bss)
    g_spis_ctrl_handle                       0x00071ddc   Data          32  hal_spi_slave.o(.bss)
    g_packet_fifo                            0x00071dfc   Data        4144  dcs_packet_fifo.o(.bss)
    __stack_limit                            0x00072e30   Data           0  startup_armcm0.o(STACK)
    __initial_sp                             0x00073e30   Data           0  startup_armcm0.o(STACK)



==============================================================================

Memory Map of the image

  Image Entry point : 0x000100c1

  Load Region LR_IROM2 (Base: 0x00010000, Size: 0x0000f7b4, Max: 0x00010000, ABSOLUTE, COMPRESSED[0x0000f2dc])

    Execution Region ER_IROM2 (Exec base: 0x00010000, Load base: 0x00010000, Size: 0x0000ec28, Max: 0x00010000, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00010000   0x00010000   0x000000c0   Data   RO          631    RESET               startup_armcm0.o
    0x000100c0   0x000100c0   0x00000000   Code   RO         2765  * .ARM.Collect$$$$00000000  mc_p.l(entry.o)
    0x000100c0   0x000100c0   0x00000004   Code   RO         3077    .ARM.Collect$$$$00000001  mc_p.l(entry2.o)
    0x000100c4   0x000100c4   0x00000004   Code   RO         3080    .ARM.Collect$$$$00000004  mc_p.l(entry5.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         3082    .ARM.Collect$$$$00000008  mc_p.l(entry7b.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         3084    .ARM.Collect$$$$0000000A  mc_p.l(entry8b.o)
    0x000100c8   0x000100c8   0x00000008   Code   RO         3085    .ARM.Collect$$$$0000000B  mc_p.l(entry9a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         3087    .ARM.Collect$$$$0000000D  mc_p.l(entry10a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         3089    .ARM.Collect$$$$0000000F  mc_p.l(entry11a.o)
    0x000100d0   0x000100d0   0x00000004   Code   RO         3078    .ARM.Collect$$$$00002712  mc_p.l(entry2.o)
    0x000100d4   0x000100d4   0x00000078   Code   RO          632    .text               startup_armcm0.o
    0x0001014c   0x0001014c   0x0000002c   Code   RO         2768    .text               mc_p.l(uidiv.o)
    0x00010178   0x00010178   0x00000028   Code   RO         2770    .text               mc_p.l(idiv.o)
    0x000101a0   0x000101a0   0x00000024   Code   RO         2772    .text               mc_p.l(memcpya.o)
    0x000101c4   0x000101c4   0x00000024   Code   RO         2774    .text               mc_p.l(memseta.o)
    0x000101e8   0x000101e8   0x000000b2   Code   RO         3039    .text               mf_p.l(fadd.o)
    0x0001029a   0x0001029a   0x0000007a   Code   RO         3041    .text               mf_p.l(fmul.o)
    0x00010314   0x00010314   0x0000007c   Code   RO         3043    .text               mf_p.l(fdiv.o)
    0x00010390   0x00010390   0x00000018   Code   RO         3045    .text               mf_p.l(fscalb.o)
    0x000103a8   0x000103a8   0x00000164   Code   RO         3047    .text               mf_p.l(dadd.o)
    0x0001050c   0x0001050c   0x000000d0   Code   RO         3049    .text               mf_p.l(dmul.o)
    0x000105dc   0x000105dc   0x000000f0   Code   RO         3051    .text               mf_p.l(ddiv.o)
    0x000106cc   0x000106cc   0x00000016   Code   RO         3053    .text               mf_p.l(fflti.o)
    0x000106e2   0x000106e2   0x0000000e   Code   RO         3055    .text               mf_p.l(ffltui.o)
    0x000106f0   0x000106f0   0x0000001c   Code   RO         3059    .text               mf_p.l(dfltui.o)
    0x0001070c   0x0001070c   0x00000032   Code   RO         3061    .text               mf_p.l(ffixi.o)
    0x0001073e   0x0001073e   0x00000028   Code   RO         3063    .text               mf_p.l(ffixui.o)
    0x00010766   0x00010766   0x00000002   PAD
    0x00010768   0x00010768   0x00000048   Code   RO         3065    .text               mf_p.l(dfixi.o)
    0x000107b0   0x000107b0   0x0000003c   Code   RO         3067    .text               mf_p.l(dfixui.o)
    0x000107ec   0x000107ec   0x00000028   Code   RO         3069    .text               mf_p.l(f2d.o)
    0x00010814   0x00010814   0x00000028   Code   RO         3071    .text               mf_p.l(cdcmple.o)
    0x0001083c   0x0001083c   0x00000014   Code   RO         3073    .text               mf_p.l(cfcmple.o)
    0x00010850   0x00010850   0x00000014   Code   RO         3075    .text               mf_p.l(cfrcmple.o)
    0x00010864   0x00010864   0x00000060   Code   RO         3092    .text               mc_p.l(uldiv.o)
    0x000108c4   0x000108c4   0x00000020   Code   RO         3094    .text               mc_p.l(llshl.o)
    0x000108e4   0x000108e4   0x00000022   Code   RO         3096    .text               mc_p.l(llushr.o)
    0x00010906   0x00010906   0x00000026   Code   RO         3098    .text               mc_p.l(llsshr.o)
    0x0001092c   0x0001092c   0x00000000   Code   RO         3107    .text               mc_p.l(iusefp.o)
    0x0001092c   0x0001092c   0x00000082   Code   RO         3108    .text               mf_p.l(fepilogue.o)
    0x000109ae   0x000109ae   0x000000be   Code   RO         3110    .text               mf_p.l(depilogue.o)
    0x00010a6c   0x00010a6c   0x000000a2   Code   RO         3114    .text               mf_p.l(dsqrt.o)
    0x00010b0e   0x00010b0e   0x00000002   PAD
    0x00010b10   0x00010b10   0x00000040   Code   RO         3116    .text               mf_p.l(dfixul.o)
    0x00010b50   0x00010b50   0x00000028   Code   RO         3118    .text               mf_p.l(cdrcmple.o)
    0x00010b78   0x00010b78   0x00000024   Code   RO         3120    .text               mc_p.l(init.o)
    0x00010b9c   0x00010b9c   0x00000056   Code   RO         3129    .text               mc_p.l(__dczerorl2.o)
    0x00010bf2   0x00010bf2   0x00000002   PAD
    0x00010bf4   0x00010bf4   0x00000018   Code   RO         2263    i.ADC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c0c   0x00010c0c   0x00000018   Code   RO         2264    i.AP_NRESET_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c24   0x00010c24   0x00000048   Code   RO          504    i.CRC16_2           app_tp_st_touch.o
    0x00010c6c   0x00010c6c   0x00000014   Code   RO         2265    i.DMA_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c80   0x00010c80   0x0000001c   Code   RO         2266    i.EXTI_INT0_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c9c   0x00010c9c   0x0000001c   Code   RO         2267    i.EXTI_INT1_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010cb8   0x00010cb8   0x0000001c   Code   RO         2268    i.EXTI_INT2_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010cd4   0x00010cd4   0x0000001c   Code   RO         2269    i.EXTI_INT3_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010cf0   0x00010cf0   0x0000001c   Code   RO         2270    i.EXTI_INT4_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010d0c   0x00010d0c   0x0000001c   Code   RO         2271    i.EXTI_INT5_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010d28   0x00010d28   0x0000001c   Code   RO         2272    i.EXTI_INT6_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010d44   0x00010d44   0x0000001c   Code   RO         2273    i.EXTI_INT7_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010d60   0x00010d60   0x00000020   Code   RO         1052    i.EncryptCheck      CVWL568_MI10PRO_HX667_TP.lib(app_tp_for_custom_s8.o)
    0x00010d80   0x00010d80   0x00000014   Code   RO         2274    i.FLSCTRL_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010d94   0x00010d94   0x00000050   Code   RO          102    i.Gpio_swire_output  ap_demo.o
    0x00010de4   0x00010de4   0x00000014   Code   RO         2275    i.HardFault_Handler  CVWL568.lib(irq_redirect .o)
    0x00010df8   0x00010df8   0x00000018   Code   RO         2276    i.I2C0_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e10   0x00010e10   0x00000018   Code   RO         2277    i.I2C1_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e28   0x00010e28   0x00000018   Code   RO         2278    i.LCDC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e40   0x00010e40   0x00000028   Code   RO         1041    i.LOG_printf        CVWL568.lib(tau_log.o)
    0x00010e68   0x00010e68   0x00000018   Code   RO         2279    i.MEMC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e80   0x00010e80   0x00000018   Code   RO         2280    i.MIPI_RX_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e98   0x00010e98   0x00000018   Code   RO         2281    i.MIPI_TX_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010eb0   0x00010eb0   0x0000001c   Code   RO         2282    i.PWMDET_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010ecc   0x00010ecc   0x0000001c   Code   RO         2283    i.SPIM_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010ee8   0x00010ee8   0x0000001c   Code   RO         2284    i.SPIS_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010f04   0x00010f04   0x0000001c   Code   RO         2285    i.SWIRE_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010f20   0x00010f20   0x00000018   Code   RO         2286    i.SysTick_Handler   CVWL568.lib(irq_redirect .o)
    0x00010f38   0x00010f38   0x00000018   Code   RO         2287    i.TIMER0_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010f50   0x00010f50   0x00000018   Code   RO         2288    i.TIMER1_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010f68   0x00010f68   0x00000018   Code   RO         2289    i.TIMER2_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010f80   0x00010f80   0x00000018   Code   RO         2290    i.TIMER3_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010f98   0x00010f98   0x0000001c   Code   RO         2632    i.UART0_IRQ_Handle  CVWL568.lib(drv_uart.o)
    0x00010fb4   0x00010fb4   0x00000002   Code   RO         2636    i.UART_DisableDma   CVWL568.lib(drv_uart.o)
    0x00010fb6   0x00010fb6   0x00000004   Code   RO         2642    i.UART_GetInstance  CVWL568.lib(drv_uart.o)
    0x00010fba   0x00010fba   0x00000002   PAD
    0x00010fbc   0x00010fbc   0x00000018   Code   RO         2291    i.UART_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010fd4   0x00010fd4   0x00000024   Code   RO         2650    i.UART_ResetRxFIFO  CVWL568.lib(drv_uart.o)
    0x00010ff8   0x00010ff8   0x00000002   Code   RO         3124    i.__scatterload_null  mc_p.l(handlers.o)
    0x00010ffa   0x00010ffa   0x00000004   Code   RO          371    i.app_tp_screen_int_lvl_low  app_tp_transfer.o
    0x00010ffe   0x00010ffe   0x00000002   PAD
    0x00011000   0x00011000   0x00000014   Data   RO         1231    .ARM.__at_0x11000   CVWL568.lib(drv_common.o)
    0x00011014   0x00011014   0x00000004   Code   RO         1840    i.drv_dsi_rx_set_inten  CVWL568.lib(drv_dsi_rx.o)
    0x00011018   0x00011018   0x00000004   Data   RO         1232    .ARM.__at_0x11018   CVWL568.lib(drv_common.o)
    0x0001101c   0x0001101c   0x00000048   Code   RO         2653    i.UART_SetBaudRate  CVWL568.lib(drv_uart.o)
    0x00011064   0x00011064   0x0000001a   Code   RO         2654    i.UART_SwitchSCLK   CVWL568.lib(drv_uart.o)
    0x0001107e   0x0001107e   0x00000134   Code   RO         2656    i.UART_TransferHandleIRQ  CVWL568.lib(drv_uart.o)
    0x000111b2   0x000111b2   0x0000001a   Code   RO         2658    i.UART_WriteBlocking  CVWL568.lib(drv_uart.o)
    0x000111cc   0x000111cc   0x000000bc   Code   RO         2659    i.UART_init         CVWL568.lib(drv_uart.o)
    0x00011288   0x00011288   0x00000018   Code   RO         2292    i.VIDC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x000112a0   0x000112a0   0x00000018   Code   RO         2293    i.VPRE_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x000112b8   0x000112b8   0x00000018   Code   RO         2294    i.WDG_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x000112d0   0x000112d0   0x00000020   Code   RO         3011    i.__0printf         mc_p.l(printfa.o)
    0x000112f0   0x000112f0   0x00000024   Code   RO         3017    i.__0vsprintf       mc_p.l(printfa.o)
    0x00011314   0x00011314   0x0000002e   Code   RO         3112    i.__ARM_clz         mf_p.l(depilogue.o)
    0x00011342   0x00011342   0x0000001a   Code   RO          732    i.__ARM_common_switch8  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001135c   0x0001135c   0x00000018   Code   RO         1552    i.__NVIC_ClearPendingIRQ  CVWL568.lib(drv_i2c_master.o)
    0x00011374   0x00011374   0x00000018   Code   RO         1676    i.__NVIC_ClearPendingIRQ  CVWL568.lib(drv_spi_master.o)
    0x0001138c   0x0001138c   0x00000020   Code   RO         2111    i.__NVIC_DisableIRQ  CVWL568.lib(drv_rxbr.o)
    0x000113ac   0x000113ac   0x00000018   Code   RO         2112    i.__NVIC_EnableIRQ  CVWL568.lib(drv_rxbr.o)
    0x000113c4   0x000113c4   0x00000044   Code   RO         2413    i.__NVIC_SetPriority  CVWL568.lib(hal_spi_slave.o)
    0x00011408   0x00011408   0x00000034   Code   RO          103    i.__NVIC_SystemReset  ap_demo.o
    0x0001143c   0x0001143c   0x0000000e   Code   RO         3123    i.__scatterload_copy  mc_p.l(handlers.o)
    0x0001144a   0x0001144a   0x0000000e   Code   RO         3125    i.__scatterload_zeroinit  mc_p.l(handlers.o)
    0x00011458   0x00011458   0x0000000c   Code   RO         3102    i.__set_errno       mc_p.l(errno.o)
    0x00011464   0x00011464   0x00000174   Code   RO         3018    i._fp_digits        mc_p.l(printfa.o)
    0x000115d8   0x000115d8   0x000006ec   Code   RO         3019    i._printf_core      mc_p.l(printfa.o)
    0x00011cc4   0x00011cc4   0x00000020   Code   RO         3020    i._printf_post_padding  mc_p.l(printfa.o)
    0x00011ce4   0x00011ce4   0x0000002c   Code   RO         3021    i._printf_pre_padding  mc_p.l(printfa.o)
    0x00011d10   0x00011d10   0x0000000a   Code   RO         3023    i._sputc            mc_p.l(printfa.o)
    0x00011d1a   0x00011d1a   0x00000002   PAD
    0x00011d1c   0x00011d1c   0x000004a0   Code   RO          104    i.ap_dcs_read       ap_demo.o
    0x000121bc   0x000121bc   0x00000278   Code   RO          105    i.ap_demo           ap_demo.o
    0x00012434   0x00012434   0x000000d0   Code   RO          106    i.ap_get_51_reg     ap_demo.o
    0x00012504   0x00012504   0x00000064   Code   RO          107    i.ap_get_67_reg     ap_demo.o
    0x00012568   0x00012568   0x00000034   Code   RO          108    i.ap_get_dcs        ap_demo.o
    0x0001259c   0x0001259c   0x00000038   Code   RO          505    i.ap_get_tp_calibration_status_01  app_tp_st_touch.o
    0x000125d4   0x000125d4   0x0000003c   Code   RO          112    i.ap_reset_cb       ap_demo.o
    0x00012610   0x00012610   0x00000054   Code   RO          116    i.ap_set_display_off  ap_demo.o
    0x00012664   0x00012664   0x00000040   Code   RO          117    i.ap_set_display_on  ap_demo.o
    0x000126a4   0x000126a4   0x0000009c   Code   RO          118    i.ap_set_enter_sleep_mode  ap_demo.o
    0x00012740   0x00012740   0x00000050   Code   RO          119    i.ap_set_exit_sleep_mode  ap_demo.o
    0x00012790   0x00012790   0x000000cc   Code   RO          506    i.ap_set_tp_calibration_04  app_tp_st_touch.o
    0x0001285c   0x0001285c   0x000000c8   Code   RO          507    i.ap_tp_st_touch_calibration  app_tp_st_touch.o
    0x00012924   0x00012924   0x00000010   Code   RO          508    i.ap_tp_st_touch_error_handler_F3  app_tp_st_touch.o
    0x00012934   0x00012934   0x00000022   Code   RO          509    i.ap_tp_st_touch_error_handler_FF  app_tp_st_touch.o
    0x00012956   0x00012956   0x00000002   PAD
    0x00012958   0x00012958   0x000000b4   Code   RO          510    i.ap_tp_st_touch_get_calibration_success_mark  app_tp_st_touch.o
    0x00012a0c   0x00012a0c   0x000000d4   Code   RO          511    i.ap_tp_st_touch_hardware_reset  app_tp_st_touch.o
    0x00012ae0   0x00012ae0   0x00000024   Code   RO          512    i.ap_tp_st_touch_scan_point_init  app_tp_st_touch.o
    0x00012b04   0x00012b04   0x000000c4   Code   RO          513    i.ap_tp_st_touch_scan_point_record_event  app_tp_st_touch.o
    0x00012bc8   0x00012bc8   0x00000060   Code   RO          514    i.ap_tp_st_touch_scan_point_record_event_exec  app_tp_st_touch.o
    0x00012c28   0x00012c28   0x0000003c   Code   RO          515    i.ap_tp_st_touch_simulate_finger_release_event  app_tp_st_touch.o
    0x00012c64   0x00012c64   0x0000001c   Code   RO         2113    i.app_ADC_IRQn_Handler  CVWL568.lib(drv_rxbr.o)
    0x00012c80   0x00012c80   0x00000024   Code   RO         1476    i.app_AP_NRESET_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00012ca4   0x00012ca4   0x0000001c   Code   RO         1477    i.app_EXTI_INT0_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00012cc0   0x00012cc0   0x0000001c   Code   RO         1478    i.app_EXTI_INT1_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00012cdc   0x00012cdc   0x0000001c   Code   RO         1479    i.app_EXTI_INT2_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00012cf8   0x00012cf8   0x0000001c   Code   RO         1480    i.app_EXTI_INT3_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00012d14   0x00012d14   0x0000001c   Code   RO         1481    i.app_EXTI_INT4_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00012d30   0x00012d30   0x0000001c   Code   RO         1482    i.app_EXTI_INT5_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00012d4c   0x00012d4c   0x0000001c   Code   RO         1483    i.app_EXTI_INT6_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00012d68   0x00012d68   0x0000001c   Code   RO         1484    i.app_EXTI_INT7_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00012d84   0x00012d84   0x00000048   Code   RO         1223    i.app_HardFault_Handler  CVWL568.lib(drv_common.o)
    0x00012dcc   0x00012dcc   0x00000018   Code   RO         1587    i.app_I2C0_IRQn_Handler  CVWL568.lib(drv_i2c_slave.o)
    0x00012de4   0x00012de4   0x00000010   Code   RO         1553    i.app_I2C1_IRQn_Handler  CVWL568.lib(drv_i2c_master.o)
    0x00012df4   0x00012df4   0x00000130   Code   RO         1124    i.app_LCDC_IRQn_Handler  CVWL568.lib(hal_internal_vsync.o)
    0x00012f24   0x00012f24   0x00000088   Code   RO         2055    i.app_MEMC_IRQn_Handler  CVWL568.lib(drv_memc.o)
    0x00012fac   0x00012fac   0x00000298   Code   RO         1825    i.app_MIPI_RX_IRQn_Handler  CVWL568.lib(drv_dsi_rx.o)
    0x00013244   0x00013244   0x000000a0   Code   RO         1883    i.app_MIPI_TX_IRQn_Handler  CVWL568.lib(drv_dsi_tx.o)
    0x000132e4   0x000132e4   0x00000048   Code   RO         2567    i.app_PWMDET_IRQn_Handler  CVWL568.lib(drv_pwm.o)
    0x0001332c   0x0001332c   0x00000030   Code   RO         1677    i.app_SPIM_IRQn_Handler  CVWL568.lib(drv_spi_master.o)
    0x0001335c   0x0001335c   0x00000200   Code   RO         2414    i.app_SPIS_IRQn_Handler  CVWL568.lib(hal_spi_slave.o)
    0x0001355c   0x0001355c   0x00000020   Code   RO         1709    i.app_SWIRE_IRQn_Handler  CVWL568.lib(drv_swire.o)
    0x0001357c   0x0001357c   0x00000018   Code   RO         1224    i.app_SysTick_Handler  CVWL568.lib(drv_common.o)
    0x00013594   0x00013594   0x0000000a   Code   RO         1759    i.app_TIMER0_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x0001359e   0x0001359e   0x0000000a   Code   RO         1760    i.app_TIMER1_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x000135a8   0x000135a8   0x0000000a   Code   RO         1761    i.app_TIMER2_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x000135b2   0x000135b2   0x0000000a   Code   RO         1762    i.app_TIMER3_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x000135bc   0x000135bc   0x00000008   Code   RO         2660    i.app_UART_IRQn_Handler  CVWL568.lib(drv_uart.o)
    0x000135c4   0x000135c4   0x0000001c   Code   RO         2184    i.app_VIDC_IRQn_Handler  CVWL568.lib(drv_vidc.o)
    0x000135e0   0x000135e0   0x0000001c   Code   RO         2114    i.app_VPRE_IRQn_Handler  CVWL568.lib(drv_rxbr.o)
    0x000135fc   0x000135fc   0x00000038   Code   RO         2719    i.app_WDG_IRQn_Handler  CVWL568.lib(drv_wdg.o)
    0x00013634   0x00013634   0x00000010   Code   RO         1338    i.app_dma_irq_handler  CVWL568.lib(drv_dma.o)
    0x00013644   0x00013644   0x00000030   Code   RO         2456    i.app_fls_ctrl_Handler  CVWL568.lib(norflash.o)
    0x00013674   0x00013674   0x000000b8   Code   RO          517    i.app_tp_calibration_exec  app_tp_st_touch.o
    0x0001372c   0x0001372c   0x0000000e   Code   RO          358    i.app_tp_i2cs_callback  app_tp_transfer.o
    0x0001373a   0x0001373a   0x00000002   PAD
    0x0001373c   0x0001373c   0x0000007c   Code   RO          359    i.app_tp_init       app_tp_transfer.o
    0x000137b8   0x000137b8   0x00000030   Code   RO          360    i.app_tp_m_read     app_tp_transfer.o
    0x000137e8   0x000137e8   0x00000008   Code   RO          361    i.app_tp_m_transfer_complate  app_tp_transfer.o
    0x000137f0   0x000137f0   0x00000010   Code   RO          362    i.app_tp_m_write    app_tp_transfer.o
    0x00013800   0x00013800   0x000002c0   Code   RO         1053    i.app_tp_phone_analysis_data  CVWL568_MI10PRO_HX667_TP.lib(app_tp_for_custom_s8.o)
    0x00013ac0   0x00013ac0   0x0000000c   Code   RO          363    i.app_tp_phone_clear_reset_on  app_tp_transfer.o
    0x00013acc   0x00013acc   0x00000010   Code   RO          365    i.app_tp_s_read     app_tp_transfer.o
    0x00013adc   0x00013adc   0x00000010   Code   RO          367    i.app_tp_s_write    app_tp_transfer.o
    0x00013aec   0x00013aec   0x00000280   Code   RO         1055    i.app_tp_screen_analysis_int  CVWL568_MI10PRO_HX667_TP.lib(app_tp_for_custom_s8.o)
    0x00013d6c   0x00013d6c   0x00000034   Code   RO          368    i.app_tp_screen_init  app_tp_transfer.o
    0x00013da0   0x00013da0   0x0000000c   Code   RO          369    i.app_tp_screen_int_callback  app_tp_transfer.o
    0x00013dac   0x00013dac   0x00000040   Code   RO          370    i.app_tp_screen_int_init  app_tp_transfer.o
    0x00013dec   0x00013dec   0x00000034   Code   RO          372    i.app_tp_transfer_phone  app_tp_transfer.o
    0x00013e20   0x00013e20   0x0000013c   Code   RO          373    i.app_tp_transfer_screen_const  app_tp_transfer.o
    0x00013f5c   0x00013f5c   0x00000174   Code   RO          374    i.app_tp_transfer_screen_int  app_tp_transfer.o
    0x000140d0   0x000140d0   0x0000000c   Code   RO          375    i.app_tp_transfer_screen_start  app_tp_transfer.o
    0x000140dc   0x000140dc   0x0000003a   Code   RO          120    i.blue_change_ccm   ap_demo.o
    0x00014116   0x00014116   0x00000002   PAD
    0x00014118   0x00014118   0x00000024   Code   RO          611    i.board_Init        board.o
    0x0001413c   0x0001413c   0x0000058c   Code   RO         1125    i.calc_framebuffer_setting  CVWL568.lib(hal_internal_vsync.o)
    0x000146c8   0x000146c8   0x000000c8   Code   RO         2754    i.ceil              m_ps.l(ceil.o)
    0x00014790   0x00014790   0x0000002c   Code   RO         1126    i.check_mipi_rx_tx_video_info  CVWL568.lib(hal_internal_vsync.o)
    0x000147bc   0x000147bc   0x00000084   Code   RO         1127    i.check_pkt_buf_rev  CVWL568.lib(hal_internal_vsync.o)
    0x00014840   0x00014840   0x00000058   Code   RO         2742    i.dcs_packet_fifo_alloc  CVWL568.lib(dcs_packet_fifo.o)
    0x00014898   0x00014898   0x00000018   Code   RO         2743    i.dcs_packet_fifo_init  CVWL568.lib(dcs_packet_fifo.o)
    0x000148b0   0x000148b0   0x00000044   Code   RO         2744    i.dcs_packet_free_fifo_header  CVWL568.lib(dcs_packet_fifo.o)
    0x000148f4   0x000148f4   0x00000024   Code   RO         2745    i.dcs_packet_get_fifo_header  CVWL568.lib(dcs_packet_fifo.o)
    0x00014918   0x00014918   0x0000002c   Code   RO         1128    i.dcs_sw_filter     CVWL568.lib(hal_internal_vsync.o)
    0x00014944   0x00014944   0x00000018   Code   RO         1033    i.delayMs           CVWL568.lib(tau_delay.o)
    0x0001495c   0x0001495c   0x00000022   Code   RO         1034    i.delayUs           CVWL568.lib(tau_delay.o)
    0x0001497e   0x0001497e   0x00000002   PAD
    0x00014980   0x00014980   0x00000038   Code   RO         1728    i.drv_ap_rst_trig_edge_detect  CVWL568.lib(drv_sys_cfg.o)
    0x000149b8   0x000149b8   0x0000000c   Code   RO         2384    i.drv_chip_info_get_info  CVWL568.lib(drv_chip_info.o)
    0x000149c4   0x000149c4   0x00000040   Code   RO         2385    i.drv_chip_info_init  CVWL568.lib(drv_chip_info.o)
    0x00014a04   0x00014a04   0x000000b0   Code   RO         2386    i.drv_chip_rx_info_check  CVWL568.lib(drv_chip_info.o)
    0x00014ab4   0x00014ab4   0x00000014   Code   RO         2387    i.drv_chip_rx_init_done  CVWL568.lib(drv_chip_info.o)
    0x00014ac8   0x00014ac8   0x00000058   Code   RO         1226    i.drv_common_enable_systick  CVWL568.lib(drv_common.o)
    0x00014b20   0x00014b20   0x00000008   Code   RO         1229    i.drv_common_system_init  CVWL568.lib(drv_common.o)
    0x00014b28   0x00014b28   0x00000010   Code   RO         1251    i.drv_crgu_config_reset_modules  CVWL568.lib(drv_crgu.o)
    0x00014b38   0x00014b38   0x00000014   Code   RO         1264    i.drv_crgu_set_ahb_pre_div  CVWL568.lib(drv_crgu.o)
    0x00014b4c   0x00014b4c   0x00000014   Code   RO         1265    i.drv_crgu_set_ahb_src  CVWL568.lib(drv_crgu.o)
    0x00014b60   0x00014b60   0x00000020   Code   RO         1268    i.drv_crgu_set_clock  CVWL568.lib(drv_crgu.o)
    0x00014b80   0x00014b80   0x00000014   Code   RO         1269    i.drv_crgu_set_dpi_mux_src  CVWL568.lib(drv_crgu.o)
    0x00014b94   0x00014b94   0x00000018   Code   RO         1270    i.drv_crgu_set_dpi_pre_div  CVWL568.lib(drv_crgu.o)
    0x00014bac   0x00014bac   0x00000014   Code   RO         1271    i.drv_crgu_set_dpi_pre_src  CVWL568.lib(drv_crgu.o)
    0x00014bc0   0x00014bc0   0x00000014   Code   RO         1272    i.drv_crgu_set_dsc_core_div  CVWL568.lib(drv_crgu.o)
    0x00014bd4   0x00014bd4   0x00000014   Code   RO         1273    i.drv_crgu_set_dsco_src  CVWL568.lib(drv_crgu.o)
    0x00014be8   0x00014be8   0x00000014   Code   RO         1274    i.drv_crgu_set_dsco_src_div  CVWL568.lib(drv_crgu.o)
    0x00014bfc   0x00014bfc   0x00000014   Code   RO         1275    i.drv_crgu_set_fb_div  CVWL568.lib(drv_crgu.o)
    0x00014c10   0x00014c10   0x00000014   Code   RO         1276    i.drv_crgu_set_fb_src  CVWL568.lib(drv_crgu.o)
    0x00014c24   0x00014c24   0x00000014   Code   RO         1279    i.drv_crgu_set_lcdc_div  CVWL568.lib(drv_crgu.o)
    0x00014c38   0x00014c38   0x00000014   Code   RO         1280    i.drv_crgu_set_lcdc_src  CVWL568.lib(drv_crgu.o)
    0x00014c4c   0x00014c4c   0x00000014   Code   RO         1281    i.drv_crgu_set_mipi_cfg_src  CVWL568.lib(drv_crgu.o)
    0x00014c60   0x00014c60   0x00000018   Code   RO         1282    i.drv_crgu_set_mipi_ref_src  CVWL568.lib(drv_crgu.o)
    0x00014c78   0x00014c78   0x00000018   Code   RO         1285    i.drv_crgu_set_reset  CVWL568.lib(drv_crgu.o)
    0x00014c90   0x00014c90   0x00000014   Code   RO         1286    i.drv_crgu_set_rxbr_div  CVWL568.lib(drv_crgu.o)
    0x00014ca4   0x00014ca4   0x00000014   Code   RO         1287    i.drv_crgu_set_rxbr_src  CVWL568.lib(drv_crgu.o)
    0x00014cb8   0x00014cb8   0x00000014   Code   RO         1289    i.drv_crgu_set_vidc_src  CVWL568.lib(drv_crgu.o)
    0x00014ccc   0x00014ccc   0x00000018   Code   RO         1342    i.drv_dma_clear_flag  CVWL568.lib(drv_dma.o)
    0x00014ce4   0x00014ce4   0x0000001c   Code   RO         1343    i.drv_dma_create_handle  CVWL568.lib(drv_dma.o)
    0x00014d00   0x00014d00   0x00000010   Code   RO         1345    i.drv_dma_disenable_channel  CVWL568.lib(drv_dma.o)
    0x00014d10   0x00014d10   0x00000010   Code   RO         1347    i.drv_dma_enable_channel  CVWL568.lib(drv_dma.o)
    0x00014d20   0x00014d20   0x00000024   Code   RO         1348    i.drv_dma_enable_channel_interrupts  CVWL568.lib(drv_dma.o)
    0x00014d44   0x00014d44   0x0000000c   Code   RO         1350    i.drv_dma_get_channel_flag  CVWL568.lib(drv_dma.o)
    0x00014d50   0x00014d50   0x00000090   Code   RO         1353    i.drv_dma_irq_handler  CVWL568.lib(drv_dma.o)
    0x00014de0   0x00014de0   0x00000012   Code   RO         1355    i.drv_dma_prepar_transfer  CVWL568.lib(drv_dma.o)
    0x00014df2   0x00014df2   0x0000001a   Code   RO         1357    i.drv_dma_set_burst  CVWL568.lib(drv_dma.o)
    0x00014e0c   0x00014e0c   0x00000006   Code   RO         1358    i.drv_dma_set_callback  CVWL568.lib(drv_dma.o)
    0x00014e12   0x00014e12   0x00000002   PAD
    0x00014e14   0x00014e14   0x00000044   Code   RO         1360    i.drv_dma_set_transfer  CVWL568.lib(drv_dma.o)
    0x00014e58   0x00014e58   0x00000036   Code   RO         2397    i.drv_dsc_dec_convert_pps_rc_parameter  CVWL568.lib(drv_dsc_dec.o)
    0x00014e8e   0x00014e8e   0x0000000c   Code   RO         2398    i.drv_dsc_dec_disable  CVWL568.lib(drv_dsc_dec.o)
    0x00014e9a   0x00014e9a   0x00000002   PAD
    0x00014e9c   0x00014e9c   0x00000074   Code   RO         2399    i.drv_dsc_dec_enable  CVWL568.lib(drv_dsc_dec.o)
    0x00014f10   0x00014f10   0x0000000a   Code   RO         2400    i.drv_dsc_dec_get_nslc  CVWL568.lib(drv_dsc_dec.o)
    0x00014f1a   0x00014f1a   0x00000028   Code   RO         2402    i.drv_dsc_dec_set_u8_pps  CVWL568.lib(drv_dsc_dec.o)
    0x00014f42   0x00014f42   0x00000002   PAD
    0x00014f44   0x00014f44   0x00000104   Code   RO         1826    i.drv_dsi_rx_calc_ipi_tx_delay  CVWL568.lib(drv_dsi_rx.o)
    0x00015048   0x00015048   0x00000040   Code   RO         1827    i.drv_dsi_rx_enable_irq  CVWL568.lib(drv_dsi_rx.o)
    0x00015088   0x00015088   0x0000000e   Code   RO         1828    i.drv_dsi_rx_get_bta_status  CVWL568.lib(drv_dsi_rx.o)
    0x00015096   0x00015096   0x00000002   PAD
    0x00015098   0x00015098   0x00000050   Code   RO         1829    i.drv_dsi_rx_get_color_bpp  CVWL568.lib(drv_dsi_rx.o)
    0x000150e8   0x000150e8   0x0000001c   Code   RO         1830    i.drv_dsi_rx_get_color_pcc  CVWL568.lib(drv_dsi_rx.o)
    0x00015104   0x00015104   0x00000008   Code   RO         1831    i.drv_dsi_rx_get_compression_en  CVWL568.lib(drv_dsi_rx.o)
    0x0001510c   0x0001510c   0x00000006   Code   RO         1832    i.drv_dsi_rx_get_max_ret_size  CVWL568.lib(drv_dsi_rx.o)
    0x00015112   0x00015112   0x0000000e   Code   RO         1836    i.drv_dsi_rx_power_up  CVWL568.lib(drv_dsi_rx.o)
    0x00015120   0x00015120   0x00000020   Code   RO         1837    i.drv_dsi_rx_set_ctrl_cfg  CVWL568.lib(drv_dsi_rx.o)
    0x00015140   0x00015140   0x00000010   Code   RO         1838    i.drv_dsi_rx_set_ddi_cfg  CVWL568.lib(drv_dsi_rx.o)
    0x00015150   0x00015150   0x00000010   Code   RO         1841    i.drv_dsi_rx_set_ipi_cfg  CVWL568.lib(drv_dsi_rx.o)
    0x00015160   0x00015160   0x00000046   Code   RO         1843    i.drv_dsi_rx_set_lane_swap  CVWL568.lib(drv_dsi_rx.o)
    0x000151a6   0x000151a6   0x00000026   Code   RO         1844    i.drv_dsi_rx_set_resp_cnt  CVWL568.lib(drv_dsi_rx.o)
    0x000151cc   0x000151cc   0x00000104   Code   RO         1845    i.drv_dsi_rx_set_up_phy  CVWL568.lib(drv_dsi_rx.o)
    0x000152d0   0x000152d0   0x0000000e   Code   RO         1846    i.drv_dsi_rx_shut_down  CVWL568.lib(drv_dsi_rx.o)
    0x000152de   0x000152de   0x00000014   Code   RO         1885    i.drv_dsi_tx_command_header  CVWL568.lib(drv_dsi_tx.o)
    0x000152f2   0x000152f2   0x0000006c   Code   RO         1886    i.drv_dsi_tx_command_mode_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x0001535e   0x0001535e   0x00000004   Code   RO         1887    i.drv_dsi_tx_command_put_payload  CVWL568.lib(drv_dsi_tx.o)
    0x00015362   0x00015362   0x00000018   Code   RO         1888    i.drv_dsi_tx_config_eotp  CVWL568.lib(drv_dsi_tx.o)
    0x0001537a   0x0001537a   0x00000008   Code   RO         1889    i.drv_dsi_tx_config_int  CVWL568.lib(drv_dsi_tx.o)
    0x00015382   0x00015382   0x00000008   Code   RO         1890    i.drv_dsi_tx_dpi_lpcmd_time  CVWL568.lib(drv_dsi_tx.o)
    0x0001538a   0x0001538a   0x0000000a   Code   RO         1891    i.drv_dsi_tx_dpi_mode  CVWL568.lib(drv_dsi_tx.o)
    0x00015394   0x00015394   0x00000024   Code   RO         1892    i.drv_dsi_tx_dpi_polarity  CVWL568.lib(drv_dsi_tx.o)
    0x000153b8   0x000153b8   0x00000004   Code   RO         1893    i.drv_dsi_tx_edpi_cmd_size  CVWL568.lib(drv_dsi_tx.o)
    0x000153bc   0x000153bc   0x00000004   Code   RO         1895    i.drv_dsi_tx_get_cmd_status  CVWL568.lib(drv_dsi_tx.o)
    0x000153c0   0x000153c0   0x00000004   Code   RO         1897    i.drv_dsi_tx_mode   CVWL568.lib(drv_dsi_tx.o)
    0x000153c4   0x000153c4   0x00000018   Code   RO         1898    i.drv_dsi_tx_phy_clock_lane_auto_lp  CVWL568.lib(drv_dsi_tx.o)
    0x000153dc   0x000153dc   0x0000001a   Code   RO         1899    i.drv_dsi_tx_phy_clock_lane_req_hs  CVWL568.lib(drv_dsi_tx.o)
    0x000153f6   0x000153f6   0x0000000c   Code   RO         1901    i.drv_dsi_tx_phy_lane_mode  CVWL568.lib(drv_dsi_tx.o)
    0x00015402   0x00015402   0x00000064   Code   RO         1905    i.drv_dsi_tx_phy_status_ready  CVWL568.lib(drv_dsi_tx.o)
    0x00015466   0x00015466   0x0000003e   Code   RO         1906    i.drv_dsi_tx_phy_status_stopstate  CVWL568.lib(drv_dsi_tx.o)
    0x000154a4   0x000154a4   0x00000134   Code   RO         1908    i.drv_dsi_tx_phy_test_setup  CVWL568.lib(drv_dsi_tx.o)
    0x000155d8   0x000155d8   0x0000001e   Code   RO         1909    i.drv_dsi_tx_phy_time_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x000155f6   0x000155f6   0x00000008   Code   RO         1913    i.drv_dsi_tx_powerup  CVWL568.lib(drv_dsi_tx.o)
    0x000155fe   0x000155fe   0x0000001c   Code   RO         1914    i.drv_dsi_tx_response_mode  CVWL568.lib(drv_dsi_tx.o)
    0x0001561a   0x0001561a   0x00000018   Code   RO         1917    i.drv_dsi_tx_set_bta_ack  CVWL568.lib(drv_dsi_tx.o)
    0x00015632   0x00015632   0x0000000c   Code   RO         1918    i.drv_dsi_tx_set_esc_div  CVWL568.lib(drv_dsi_tx.o)
    0x0001563e   0x0001563e   0x00000002   PAD
    0x00015640   0x00015640   0x00000040   Code   RO         1919    i.drv_dsi_tx_set_int  CVWL568.lib(drv_dsi_tx.o)
    0x00015680   0x00015680   0x00000010   Code   RO         1920    i.drv_dsi_tx_set_time_out_div  CVWL568.lib(drv_dsi_tx.o)
    0x00015690   0x00015690   0x00000008   Code   RO         1921    i.drv_dsi_tx_set_video_chunk  CVWL568.lib(drv_dsi_tx.o)
    0x00015698   0x00015698   0x00000022   Code   RO         1922    i.drv_dsi_tx_set_video_timing  CVWL568.lib(drv_dsi_tx.o)
    0x000156ba   0x000156ba   0x00000008   Code   RO         1924    i.drv_dsi_tx_shutdown  CVWL568.lib(drv_dsi_tx.o)
    0x000156c2   0x000156c2   0x00000026   Code   RO         1925    i.drv_dsi_tx_timeout_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x000156e8   0x000156e8   0x000000aa   Code   RO         1928    i.drv_dsi_tx_video_mode_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x00015792   0x00015792   0x00000016   Code   RO         1929    i.drv_dsi_tx_video_mode_disable_hact_cmd  CVWL568.lib(drv_dsi_tx.o)
    0x000157a8   0x000157a8   0x00000018   Code   RO         1930    i.drv_dsi_tx_video_mode_set_lp_cmd  CVWL568.lib(drv_dsi_tx.o)
    0x000157c0   0x000157c0   0x0000002e   Code   RO         2335    i.drv_efuse_enter_inactive  CVWL568.lib(drv_efuse.o)
    0x000157ee   0x000157ee   0x0000000c   Code   RO         2338    i.drv_efuse_int_enable  CVWL568.lib(drv_efuse.o)
    0x000157fa   0x000157fa   0x00000032   Code   RO         2339    i.drv_efuse_read    CVWL568.lib(drv_efuse.o)
    0x0001582c   0x0001582c   0x00000018   Code   RO         2340    i.drv_efuse_read_req  CVWL568.lib(drv_efuse.o)
    0x00015844   0x00015844   0x00000018   Code   RO         1485    i.drv_gpio_get_input_data  CVWL568.lib(drv_gpio.o)
    0x0001585c   0x0001585c   0x0000000c   Code   RO         1487    i.drv_gpio_register_ap_reset_callback  CVWL568.lib(drv_gpio.o)
    0x00015868   0x00015868   0x00000014   Code   RO         1488    i.drv_gpio_register_callback  CVWL568.lib(drv_gpio.o)
    0x0001587c   0x0001587c   0x00000050   Code   RO         1490    i.drv_gpio_set_int  CVWL568.lib(drv_gpio.o)
    0x000158cc   0x000158cc   0x00000020   Code   RO         1491    i.drv_gpio_set_ioe  CVWL568.lib(drv_gpio.o)
    0x000158ec   0x000158ec   0x00000010   Code   RO         1492    i.drv_gpio_set_mode0  CVWL568.lib(drv_gpio.o)
    0x000158fc   0x000158fc   0x00000010   Code   RO         1493    i.drv_gpio_set_mode1  CVWL568.lib(drv_gpio.o)
    0x0001590c   0x0001590c   0x00000010   Code   RO         1494    i.drv_gpio_set_mode2  CVWL568.lib(drv_gpio.o)
    0x0001591c   0x0001591c   0x00000010   Code   RO         1495    i.drv_gpio_set_mode3  CVWL568.lib(drv_gpio.o)
    0x0001592c   0x0001592c   0x00000020   Code   RO          842    i.drv_gpio_set_output_data  CVWL568.lib(hal_gpio.o)
    0x0001594c   0x0001594c   0x00000130   Code   RO         1496    i.drv_gpio_set_pull_state  CVWL568.lib(drv_gpio.o)
    0x00015a7c   0x00015a7c   0x0000000c   Code   RO         1588    i.drv_i2c0_set_callback  CVWL568.lib(drv_i2c_slave.o)
    0x00015a88   0x00015a88   0x0000000c   Code   RO         1554    i.drv_i2c1_set_callback  CVWL568.lib(drv_i2c_master.o)
    0x00015a94   0x00015a94   0x00000034   Code   RO         1528    i.drv_i2c_dma_callback  CVWL568.lib(drv_i2c_dma.o)
    0x00015ac8   0x00015ac8   0x000000ac   Code   RO         1529    i.drv_i2c_dma_init  CVWL568.lib(drv_i2c_dma.o)
    0x00015b74   0x00015b74   0x0000001a   Code   RO         1530    i.drv_i2c_enable_rx_dma  CVWL568.lib(drv_i2c_dma.o)
    0x00015b8e   0x00015b8e   0x00000018   Code   RO         1531    i.drv_i2c_enable_tx_dma  CVWL568.lib(drv_i2c_dma.o)
    0x00015ba6   0x00015ba6   0x00000002   PAD
    0x00015ba8   0x00015ba8   0x00000060   Code   RO         1556    i.drv_i2c_m_clear_it_pending_bit  CVWL568.lib(drv_i2c_master.o)
    0x00015c08   0x00015c08   0x00000010   Code   RO         1559    i.drv_i2c_m_enable  CVWL568.lib(drv_i2c_master.o)
    0x00015c18   0x00015c18   0x00000038   Code   RO         1560    i.drv_i2c_m_enable_intr  CVWL568.lib(drv_i2c_master.o)
    0x00015c50   0x00015c50   0x0000008c   Code   RO         1566    i.drv_i2c_master_init  CVWL568.lib(drv_i2c_master.o)
    0x00015cdc   0x00015cdc   0x0000005c   Code   RO         1532    i.drv_i2c_master_read_dma  CVWL568.lib(drv_i2c_dma.o)
    0x00015d38   0x00015d38   0x0000003c   Code   RO         1533    i.drv_i2c_master_write_dma  CVWL568.lib(drv_i2c_dma.o)
    0x00015d74   0x00015d74   0x0000003e   Code   RO         1534    i.drv_i2c_master_write_read_cmd  CVWL568.lib(drv_i2c_dma.o)
    0x00015db2   0x00015db2   0x00000042   Code   RO         1589    i.drv_i2c_s_clear_it_pending_bit  CVWL568.lib(drv_i2c_slave.o)
    0x00015df4   0x00015df4   0x00000004   Code   RO         1590    i.drv_i2c_s_config_intr  CVWL568.lib(drv_i2c_slave.o)
    0x00015df8   0x00015df8   0x00000008   Code   RO         1591    i.drv_i2c_s_enable  CVWL568.lib(drv_i2c_slave.o)
    0x00015e00   0x00015e00   0x00000014   Code   RO         1592    i.drv_i2c_s_get_fifo_status  CVWL568.lib(drv_i2c_slave.o)
    0x00015e14   0x00015e14   0x00000050   Code   RO         1595    i.drv_i2c_s_set_intr  CVWL568.lib(drv_i2c_slave.o)
    0x00015e64   0x00015e64   0x0000001c   Code   RO         1596    i.drv_i2c_s_write_data  CVWL568.lib(drv_i2c_slave.o)
    0x00015e80   0x00015e80   0x00000058   Code   RO         1535    i.drv_i2c_set_dma_irq_callback  CVWL568.lib(drv_i2c_dma.o)
    0x00015ed8   0x00015ed8   0x00000032   Code   RO         1597    i.drv_i2c_slave_init  CVWL568.lib(drv_i2c_slave.o)
    0x00015f0a   0x00015f0a   0x00000002   PAD
    0x00015f0c   0x00015f0c   0x00000018   Code   RO         1536    i.drv_i2c_slave_write_dma  CVWL568.lib(drv_i2c_dma.o)
    0x00015f24   0x00015f24   0x00000018   Code   RO         1997    i.drv_lcdc_config_bypass  CVWL568.lib(drv_lcdc.o)
    0x00015f3c   0x00015f3c   0x00000030   Code   RO         1998    i.drv_lcdc_config_ccm  CVWL568.lib(drv_lcdc.o)
    0x00015f6c   0x00015f6c   0x00000016   Code   RO         1999    i.drv_lcdc_config_disp_mode  CVWL568.lib(drv_lcdc.o)
    0x00015f82   0x00015f82   0x00000024   Code   RO         2000    i.drv_lcdc_config_dpi_polarity  CVWL568.lib(drv_lcdc.o)
    0x00015fa6   0x00015fa6   0x00000026   Code   RO         2001    i.drv_lcdc_config_dpi_timing  CVWL568.lib(drv_lcdc.o)
    0x00015fcc   0x00015fcc   0x00000016   Code   RO         2002    i.drv_lcdc_config_edpi_mode  CVWL568.lib(drv_lcdc.o)
    0x00015fe2   0x00015fe2   0x00000016   Code   RO         2003    i.drv_lcdc_config_endianness  CVWL568.lib(drv_lcdc.o)
    0x00015ff8   0x00015ff8   0x0000000c   Code   RO         2004    i.drv_lcdc_config_input_size  CVWL568.lib(drv_lcdc.o)
    0x00016004   0x00016004   0x0000001e   Code   RO         2005    i.drv_lcdc_config_int  CVWL568.lib(drv_lcdc.o)
    0x00016022   0x00016022   0x00000022   Code   RO         2006    i.drv_lcdc_config_int_single  CVWL568.lib(drv_lcdc.o)
    0x00016044   0x00016044   0x00000022   Code   RO         2007    i.drv_lcdc_config_overwrite  CVWL568.lib(drv_lcdc.o)
    0x00016066   0x00016066   0x0000000c   Code   RO         2008    i.drv_lcdc_config_overwrite_rgb  CVWL568.lib(drv_lcdc.o)
    0x00016072   0x00016072   0x0000001a   Code   RO         2009    i.drv_lcdc_config_partial_display_area  CVWL568.lib(drv_lcdc.o)
    0x0001608c   0x0001608c   0x00000022   Code   RO         2010    i.drv_lcdc_config_partial_display_enable  CVWL568.lib(drv_lcdc.o)
    0x000160ae   0x000160ae   0x0000001a   Code   RO         2012    i.drv_lcdc_config_scale_up_coef  CVWL568.lib(drv_lcdc.o)
    0x000160c8   0x000160c8   0x0000000c   Code   RO         2013    i.drv_lcdc_config_scale_up_step  CVWL568.lib(drv_lcdc.o)
    0x000160d4   0x000160d4   0x0000004c   Code   RO         2014    i.drv_lcdc_config_src_parameter  CVWL568.lib(drv_lcdc.o)
    0x00016120   0x00016120   0x00000006   Code   RO         2015    i.drv_lcdc_config_thresh  CVWL568.lib(drv_lcdc.o)
    0x00016126   0x00016126   0x00000012   Code   RO         2016    i.drv_lcdc_ctrl_flow  CVWL568.lib(drv_lcdc.o)
    0x00016138   0x00016138   0x00000020   Code   RO         2018    i.drv_lcdc_enable_shadow_reg  CVWL568.lib(drv_lcdc.o)
    0x00016158   0x00016158   0x00000040   Code   RO         2019    i.drv_lcdc_set_int  CVWL568.lib(drv_lcdc.o)
    0x00016198   0x00016198   0x00000018   Code   RO         2020    i.drv_lcdc_set_prefetch  CVWL568.lib(drv_lcdc.o)
    0x000161b0   0x000161b0   0x00000014   Code   RO         2021    i.drv_lcdc_set_video_hw_mode  CVWL568.lib(drv_lcdc.o)
    0x000161c4   0x000161c4   0x00000020   Code   RO         2022    i.drv_lcdc_start    CVWL568.lib(drv_lcdc.o)
    0x000161e4   0x000161e4   0x0000000c   Code   RO         2056    i.drv_memc_clear_status  CVWL568.lib(drv_memc.o)
    0x000161f0   0x000161f0   0x00000040   Code   RO         2057    i.drv_memc_enable_irq  CVWL568.lib(drv_memc.o)
    0x00016230   0x00016230   0x0000000c   Code   RO         2058    i.drv_memc_gen_a_tear_signal  CVWL568.lib(drv_memc.o)
    0x0001623c   0x0001623c   0x00000012   Code   RO         2059    i.drv_memc_get_status  CVWL568.lib(drv_memc.o)
    0x0001624e   0x0001624e   0x00000010   Code   RO         2060    i.drv_memc_rate_transfer_sel  CVWL568.lib(drv_memc.o)
    0x0001625e   0x0001625e   0x0000000e   Code   RO         2061    i.drv_memc_sel_vsync  CVWL568.lib(drv_memc.o)
    0x0001626c   0x0001626c   0x00000014   Code   RO         2062    i.drv_memc_set_active_height  CVWL568.lib(drv_memc.o)
    0x00016280   0x00016280   0x0000000c   Code   RO         2063    i.drv_memc_set_data_mode  CVWL568.lib(drv_memc.o)
    0x0001628c   0x0001628c   0x00000010   Code   RO         2066    i.drv_memc_set_double_buffer  CVWL568.lib(drv_memc.o)
    0x0001629c   0x0001629c   0x00000012   Code   RO         2067    i.drv_memc_set_double_buffer_reverse  CVWL568.lib(drv_memc.o)
    0x000162ae   0x000162ae   0x00000010   Code   RO         2069    i.drv_memc_set_fs_en_conditions  CVWL568.lib(drv_memc.o)
    0x000162be   0x000162be   0x00000014   Code   RO         2070    i.drv_memc_set_inten  CVWL568.lib(drv_memc.o)
    0x000162d2   0x000162d2   0x00000002   PAD
    0x000162d4   0x000162d4   0x00000018   Code   RO         2071    i.drv_memc_set_lcdc_st_conditions  CVWL568.lib(drv_memc.o)
    0x000162ec   0x000162ec   0x0000001a   Code   RO         2072    i.drv_memc_set_ltpo_mode  CVWL568.lib(drv_memc.o)
    0x00016306   0x00016306   0x0000000e   Code   RO         2076    i.drv_memc_set_tear_mode  CVWL568.lib(drv_memc.o)
    0x00016314   0x00016314   0x00000028   Code   RO         2077    i.drv_memc_set_tear_waveform  CVWL568.lib(drv_memc.o)
    0x0001633c   0x0001633c   0x0000000e   Code   RO         2079    i.drv_memc_set_vidc_sync_cnt  CVWL568.lib(drv_memc.o)
    0x0001634a   0x0001634a   0x00000002   PAD
    0x0001634c   0x0001634c   0x00000008   Code   RO         1614    i.drv_param_init_get_ccm  CVWL568.lib(drv_param_init.o)
    0x00016354   0x00016354   0x00000014   Code   RO         1615    i.drv_param_init_get_scld_filter_h  CVWL568.lib(drv_param_init.o)
    0x00016368   0x00016368   0x00000014   Code   RO         1616    i.drv_param_init_get_scld_filter_v  CVWL568.lib(drv_param_init.o)
    0x0001637c   0x0001637c   0x00000008   Code   RO         1617    i.drv_param_init_get_sclu_filter  CVWL568.lib(drv_param_init.o)
    0x00016384   0x00016384   0x00000014   Code   RO         1618    i.drv_param_init_set_ccm  CVWL568.lib(drv_param_init.o)
    0x00016398   0x00016398   0x00000064   Code   RO         1619    i.drv_param_init_set_scld_filter  CVWL568.lib(drv_param_init.o)
    0x000163fc   0x000163fc   0x00000024   Code   RO         1621    i.drv_param_p2r_filter_init  CVWL568.lib(drv_param_init.o)
    0x00016420   0x00016420   0x00000010   Code   RO         2356    i.drv_phy_enable_calibration  CVWL568.lib(drv_phy_common.o)
    0x00016430   0x00016430   0x0000003c   Code   RO         2357    i.drv_phy_get_calibration  CVWL568.lib(drv_phy_common.o)
    0x0001646c   0x0001646c   0x00000060   Code   RO         2358    i.drv_phy_get_pll_para  CVWL568.lib(drv_phy_common.o)
    0x000164cc   0x000164cc   0x00000054   Code   RO         2359    i.drv_phy_get_rate_para  CVWL568.lib(drv_phy_common.o)
    0x00016520   0x00016520   0x00000010   Code   RO         2360    i.drv_phy_test_clear  CVWL568.lib(drv_phy_common.o)
    0x00016530   0x00016530   0x00000018   Code   RO         2361    i.drv_phy_test_lock  CVWL568.lib(drv_phy_common.o)
    0x00016548   0x00016548   0x00000020   Code   RO         2363    i.drv_phy_test_write_1_byte  CVWL568.lib(drv_phy_common.o)
    0x00016568   0x00016568   0x00000026   Code   RO         2364    i.drv_phy_test_write_2_byte  CVWL568.lib(drv_phy_common.o)
    0x0001658e   0x0001658e   0x0000001e   Code   RO         2365    i.drv_phy_test_write_code  CVWL568.lib(drv_phy_common.o)
    0x000165ac   0x000165ac   0x00000020   Code   RO         2366    i.drv_phy_test_write_data  CVWL568.lib(drv_phy_common.o)
    0x000165cc   0x000165cc   0x00000020   Code   RO         1637    i.drv_pwr_set_cp_mode  CVWL568.lib(drv_pwr.o)
    0x000165ec   0x000165ec   0x00000018   Code   RO         1639    i.drv_pwr_set_pvd_mode  CVWL568.lib(drv_pwr.o)
    0x00016604   0x00016604   0x00000038   Code   RO         1640    i.drv_pwr_set_system_clk_src  CVWL568.lib(drv_pwr.o)
    0x0001663c   0x0001663c   0x0000000c   Code   RO         1847    i.drv_rx_phy_test_clear  CVWL568.lib(drv_dsi_rx.o)
    0x00016648   0x00016648   0x00000010   Code   RO         1848    i.drv_rx_phy_test_lock  CVWL568.lib(drv_dsi_rx.o)
    0x00016658   0x00016658   0x00000014   Code   RO         1850    i.drv_rx_phy_test_write_1_byte  CVWL568.lib(drv_dsi_rx.o)
    0x0001666c   0x0001666c   0x00000016   Code   RO         1851    i.drv_rx_phy_test_write_2_byte  CVWL568.lib(drv_dsi_rx.o)
    0x00016682   0x00016682   0x0000000a   Code   RO         2115    i.drv_rxbr_clear_pkt_buffer  CVWL568.lib(drv_rxbr.o)
    0x0001668c   0x0001668c   0x00000004   Code   RO         2116    i.drv_rxbr_clear_status0  CVWL568.lib(drv_rxbr.o)
    0x00016690   0x00016690   0x0000005a   Code   RO         2118    i.drv_rxbr_enable_irq  CVWL568.lib(drv_rxbr.o)
    0x000166ea   0x000166ea   0x00000002   PAD
    0x000166ec   0x000166ec   0x00000014   Code   RO         2119    i.drv_rxbr_frame_drop_cfg  CVWL568.lib(drv_rxbr.o)
    0x00016700   0x00016700   0x00000064   Code   RO         2120    i.drv_rxbr_get_clk  CVWL568.lib(drv_rxbr.o)
    0x00016764   0x00016764   0x00000004   Code   RO         2121    i.drv_rxbr_get_col_addr  CVWL568.lib(drv_rxbr.o)
    0x00016768   0x00016768   0x00000012   Code   RO         1129    i.drv_rxbr_get_int_source  CVWL568.lib(hal_internal_vsync.o)
    0x0001677a   0x0001677a   0x00000004   Code   RO         2124    i.drv_rxbr_get_page_addr  CVWL568.lib(drv_rxbr.o)
    0x0001677e   0x0001677e   0x0000000c   Code   RO         2126    i.drv_rxbr_get_pkt_buf_error_status  CVWL568.lib(drv_rxbr.o)
    0x0001678a   0x0001678a   0x00000012   Code   RO         1130    i.drv_rxbr_get_status0  CVWL568.lib(hal_internal_vsync.o)
    0x0001679c   0x0001679c   0x00000016   Code   RO         1131    i.drv_rxbr_get_status1  CVWL568.lib(hal_internal_vsync.o)
    0x000167b2   0x000167b2   0x0000000c   Code   RO         2128    i.drv_rxbr_hline_rcv1_cfg  CVWL568.lib(drv_rxbr.o)
    0x000167be   0x000167be   0x00000008   Code   RO         2129    i.drv_rxbr_hline_rcv_cfg  CVWL568.lib(drv_rxbr.o)
    0x000167c6   0x000167c6   0x00000002   PAD
    0x000167c8   0x000167c8   0x0000000c   Code   RO         2130    i.drv_rxbr_register_irq0_callback  CVWL568.lib(drv_rxbr.o)
    0x000167d4   0x000167d4   0x0000000c   Code   RO         2131    i.drv_rxbr_register_irq1_callback  CVWL568.lib(drv_rxbr.o)
    0x000167e0   0x000167e0   0x00000014   Code   RO         2132    i.drv_rxbr_set_ack_pkt_header  CVWL568.lib(drv_rxbr.o)
    0x000167f4   0x000167f4   0x00000014   Code   RO         2135    i.drv_rxbr_set_color_format  CVWL568.lib(drv_rxbr.o)
    0x00016808   0x00016808   0x00000012   Code   RO         2137    i.drv_rxbr_set_filter_regs  CVWL568.lib(drv_rxbr.o)
    0x0001681a   0x0001681a   0x00000014   Code   RO         2138    i.drv_rxbr_set_inten  CVWL568.lib(drv_rxbr.o)
    0x0001682e   0x0001682e   0x00000010   Code   RO         2139    i.drv_rxbr_set_ltpo_drop_th  CVWL568.lib(drv_rxbr.o)
    0x0001683e   0x0001683e   0x00000026   Code   RO         2141    i.drv_rxbr_set_usr_cfg  CVWL568.lib(drv_rxbr.o)
    0x00016864   0x00016864   0x00000008   Code   RO         2142    i.drv_rxbr_set_usr_col  CVWL568.lib(drv_rxbr.o)
    0x0001686c   0x0001686c   0x00000008   Code   RO         2143    i.drv_rxbr_set_usr_row  CVWL568.lib(drv_rxbr.o)
    0x00016874   0x00016874   0x00000020   Code   RO         1685    i.drv_spi_m_read_data  CVWL568.lib(drv_spi_master.o)
    0x00016894   0x00016894   0x0000001c   Code   RO         1710    i.drv_swire_enable  CVWL568.lib(drv_swire.o)
    0x000168b0   0x000168b0   0x00000054   Code   RO         1713    i.drv_swire_set_int  CVWL568.lib(drv_swire.o)
    0x00016904   0x00016904   0x0000001c   Code   RO         1714    i.drv_swire_set_power_down  CVWL568.lib(drv_swire.o)
    0x00016920   0x00016920   0x0000000c   Code   RO         1729    i.drv_sys_cfg_clear_all_int  CVWL568.lib(drv_sys_cfg.o)
    0x0001692c   0x0001692c   0x00000028   Code   RO         1730    i.drv_sys_cfg_clear_pending  CVWL568.lib(drv_sys_cfg.o)
    0x00016954   0x00016954   0x00000018   Code   RO         1733    i.drv_sys_cfg_sel_ap_rst_lvl_trig  CVWL568.lib(drv_sys_cfg.o)
    0x0001696c   0x0001696c   0x0000001c   Code   RO         1734    i.drv_sys_cfg_sel_ap_rst_trig  CVWL568.lib(drv_sys_cfg.o)
    0x00016988   0x00016988   0x00000024   Code   RO         1735    i.drv_sys_cfg_sel_gpio_group  CVWL568.lib(drv_sys_cfg.o)
    0x000169ac   0x000169ac   0x00000024   Code   RO         1736    i.drv_sys_cfg_sel_int_trig  CVWL568.lib(drv_sys_cfg.o)
    0x000169d0   0x000169d0   0x00000010   Code   RO         1738    i.drv_sys_cfg_set_dma_rx_req  CVWL568.lib(drv_sys_cfg.o)
    0x000169e0   0x000169e0   0x00000010   Code   RO         1739    i.drv_sys_cfg_set_dma_tx_req  CVWL568.lib(drv_sys_cfg.o)
    0x000169f0   0x000169f0   0x00000024   Code   RO         1740    i.drv_sys_cfg_set_int  CVWL568.lib(drv_sys_cfg.o)
    0x00016a14   0x00016a14   0x0000001a   Code   RO         1763    i.drv_timer_clear_status_flags  CVWL568.lib(drv_timer.o)
    0x00016a2e   0x00016a2e   0x00000020   Code   RO         1764    i.drv_timer_enable  CVWL568.lib(drv_timer.o)
    0x00016a4e   0x00016a4e   0x00000002   PAD
    0x00016a50   0x00016a50   0x00000010   Code   RO         1765    i.drv_timer_get_instance  CVWL568.lib(drv_timer.o)
    0x00016a60   0x00016a60   0x00000010   Code   RO         1766    i.drv_timer_get_prescaler  CVWL568.lib(drv_timer.o)
    0x00016a70   0x00016a70   0x00000044   Code   RO         1768    i.drv_timer_handle_interrupt  CVWL568.lib(drv_timer.o)
    0x00016ab4   0x00016ab4   0x00000014   Code   RO         1769    i.drv_timer_register_callback  CVWL568.lib(drv_timer.o)
    0x00016ac8   0x00016ac8   0x00000010   Code   RO         1770    i.drv_timer_set_compare_val  CVWL568.lib(drv_timer.o)
    0x00016ad8   0x00016ad8   0x00000054   Code   RO         1771    i.drv_timer_set_int  CVWL568.lib(drv_timer.o)
    0x00016b2c   0x00016b2c   0x00000028   Code   RO         1772    i.drv_timer_set_prescaler  CVWL568.lib(drv_timer.o)
    0x00016b54   0x00016b54   0x00000010   Code   RO         1773    i.drv_timer_set_repeat  CVWL568.lib(drv_timer.o)
    0x00016b64   0x00016b64   0x0000000a   Code   RO         1931    i.drv_tx_phy_test_clear  CVWL568.lib(drv_dsi_tx.o)
    0x00016b6e   0x00016b6e   0x0000001c   Code   RO         1932    i.drv_tx_phy_test_enter  CVWL568.lib(drv_dsi_tx.o)
    0x00016b8a   0x00016b8a   0x0000001c   Code   RO         1933    i.drv_tx_phy_test_exit  CVWL568.lib(drv_dsi_tx.o)
    0x00016ba6   0x00016ba6   0x00000012   Code   RO         1935    i.drv_tx_phy_test_write_1_byte  CVWL568.lib(drv_dsi_tx.o)
    0x00016bb8   0x00016bb8   0x00000014   Code   RO         1936    i.drv_tx_phy_test_write_2_byte  CVWL568.lib(drv_dsi_tx.o)
    0x00016bcc   0x00016bcc   0x00000010   Code   RO         1937    i.drv_tx_phy_test_write_code  CVWL568.lib(drv_dsi_tx.o)
    0x00016bdc   0x00016bdc   0x00000008   Code   RO         2185    i.drv_vidc_clear_irq  CVWL568.lib(drv_vidc.o)
    0x00016be4   0x00016be4   0x00000018   Code   RO         2189    i.drv_vidc_enable   CVWL568.lib(drv_vidc.o)
    0x00016bfc   0x00016bfc   0x00000040   Code   RO         2190    i.drv_vidc_enable_irq  CVWL568.lib(drv_vidc.o)
    0x00016c3c   0x00016c3c   0x00000012   Code   RO         2192    i.drv_vidc_get_irq_status  CVWL568.lib(drv_vidc.o)
    0x00016c4e   0x00016c4e   0x00000002   PAD
    0x00016c50   0x00016c50   0x00000028   Code   RO         2196    i.drv_vidc_init_module_enable  CVWL568.lib(drv_vidc.o)
    0x00016c78   0x00016c78   0x0000000c   Code   RO         2197    i.drv_vidc_register_callback  CVWL568.lib(drv_vidc.o)
    0x00016c84   0x00016c84   0x00000006   Code   RO         2198    i.drv_vidc_reset    CVWL568.lib(drv_vidc.o)
    0x00016c8a   0x00016c8a   0x0000003c   Code   RO         2200    i.drv_vidc_set_dst_parameter  CVWL568.lib(drv_vidc.o)
    0x00016cc6   0x00016cc6   0x00000014   Code   RO         2204    i.drv_vidc_set_irqen  CVWL568.lib(drv_vidc.o)
    0x00016cda   0x00016cda   0x00000010   Code   RO         2205    i.drv_vidc_set_mirror  CVWL568.lib(drv_vidc.o)
    0x00016cea   0x00016cea   0x00000008   Code   RO         2208    i.drv_vidc_set_p2r_hcoef0  CVWL568.lib(drv_vidc.o)
    0x00016cf2   0x00016cf2   0x00000026   Code   RO         2209    i.drv_vidc_set_p2r_hinitb  CVWL568.lib(drv_vidc.o)
    0x00016d18   0x00016d18   0x00000026   Code   RO         2210    i.drv_vidc_set_p2r_hinitr  CVWL568.lib(drv_vidc.o)
    0x00016d3e   0x00016d3e   0x00000002   PAD
    0x00016d40   0x00016d40   0x00000018   Code   RO         2211    i.drv_vidc_set_pentile_swap  CVWL568.lib(drv_vidc.o)
    0x00016d58   0x00016d58   0x0000000a   Code   RO         2212    i.drv_vidc_set_pu_ctrl  CVWL568.lib(drv_vidc.o)
    0x00016d62   0x00016d62   0x00000010   Code   RO         2213    i.drv_vidc_set_rotation  CVWL568.lib(drv_vidc.o)
    0x00016d72   0x00016d72   0x0000000a   Code   RO         2214    i.drv_vidc_set_scld_hcoef0  CVWL568.lib(drv_vidc.o)
    0x00016d7c   0x00016d7c   0x0000000a   Code   RO         2215    i.drv_vidc_set_scld_hcoef1  CVWL568.lib(drv_vidc.o)
    0x00016d86   0x00016d86   0x00000012   Code   RO         2216    i.drv_vidc_set_scld_step  CVWL568.lib(drv_vidc.o)
    0x00016d98   0x00016d98   0x0000000a   Code   RO         2217    i.drv_vidc_set_scld_vcoef0  CVWL568.lib(drv_vidc.o)
    0x00016da2   0x00016da2   0x0000000a   Code   RO         2218    i.drv_vidc_set_scld_vcoef1  CVWL568.lib(drv_vidc.o)
    0x00016dac   0x00016dac   0x00000016   Code   RO         2219    i.drv_vidc_set_src_parameter  CVWL568.lib(drv_vidc.o)
    0x00016dc2   0x00016dc2   0x00000002   PAD
    0x00016dc4   0x00016dc4   0x00000010   Code   RO         2720    i.drv_wdg_clear_counter  CVWL568.lib(drv_wdg.o)
    0x00016dd4   0x00016dd4   0x00000010   Code   RO         2721    i.drv_wdg_clear_edge_flag  CVWL568.lib(drv_wdg.o)
    0x00016de4   0x00016de4   0x00000010   Code   RO         2724    i.drv_wdg_read_edge_flag  CVWL568.lib(drv_wdg.o)
    0x00016df4   0x00016df4   0x00000040   Code   RO         2727    i.drv_wdg_set_int   CVWL568.lib(drv_wdg.o)
    0x00016e34   0x00016e34   0x00000014   Code   RO          121    i.finger_calibration_init  ap_demo.o
    0x00016e48   0x00016e48   0x0000000a   Code   RO         1397    i.fls_clr_interrupt_flag  CVWL568.lib(drv_fls.o)
    0x00016e52   0x00016e52   0x00000014   Code   RO         1043    i.fputc             CVWL568.lib(tau_log.o)
    0x00016e66   0x00016e66   0x00000002   PAD
    0x00016e68   0x00016e68   0x00000058   Code   RO          638    i.hal_dsi_rx_ctrl_ack_long_cmd  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016ec0   0x00016ec0   0x00000034   Code   RO          640    i.hal_dsi_rx_ctrl_create_handle  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016ef4   0x00016ef4   0x000000b0   Code   RO          642    i.hal_dsi_rx_ctrl_deinit  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016fa4   0x00016fa4   0x00000028   Code   RO          644    i.hal_dsi_rx_ctrl_dsc_async_handler  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016fcc   0x00016fcc   0x00000028   Code   RO          646    i.hal_dsi_rx_ctrl_gen_a_tear_signal  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016ff4   0x00016ff4   0x00000028   Code   RO          648    i.hal_dsi_rx_ctrl_get_max_ret_size  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001701c   0x0001701c   0x00000098   Code   RO          650    i.hal_dsi_rx_ctrl_init  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000170b4   0x000170b4   0x000001a4   Code   RO          651    i.hal_dsi_rx_ctrl_init_clk  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017258   0x00017258   0x000000d8   Code   RO          652    i.hal_dsi_rx_ctrl_init_dsi_rx  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017330   0x00017330   0x00000160   Code   RO          653    i.hal_dsi_rx_ctrl_init_memc  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017490   0x00017490   0x00000150   Code   RO          654    i.hal_dsi_rx_ctrl_init_rxbr  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000175e0   0x000175e0   0x0000022c   Code   RO          655    i.hal_dsi_rx_ctrl_init_vidc  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001780c   0x0001780c   0x0000003c   Code   RO          656    i.hal_dsi_rx_ctrl_pre_init_pps  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017848   0x00017848   0x000000f0   Code   RO          660    i.hal_dsi_rx_ctrl_send_ack_cmd  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017938   0x00017938   0x0000006c   Code   RO          663    i.hal_dsi_rx_ctrl_set_cus_scld_filter  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000179a4   0x000179a4   0x00000034   Code   RO          667    i.hal_dsi_rx_ctrl_set_hw_tear_mode  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000179d8   0x000179d8   0x00000038   Code   RO          668    i.hal_dsi_rx_ctrl_set_ipi_cfg  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017a10   0x00017a10   0x00000072   Code   RO          673    i.hal_dsi_rx_ctrl_set_rxbr_clk  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017a82   0x00017a82   0x00000002   PAD
    0x00017a84   0x00017a84   0x00000034   Code   RO          674    i.hal_dsi_rx_ctrl_set_sw_tear_mode  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017ab8   0x00017ab8   0x0000000e   Code   RO          676    i.hal_dsi_rx_ctrl_set_tear_mode_ex  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017ac6   0x00017ac6   0x00000002   PAD
    0x00017ac8   0x00017ac8   0x0000003c   Code   RO          677    i.hal_dsi_rx_ctrl_start  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017b04   0x00017b04   0x0000003c   Code   RO          678    i.hal_dsi_rx_ctrl_stop  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017b40   0x00017b40   0x00000020   Code   RO          680    i.hal_dsi_rx_ctrl_toggle_resolution  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017b60   0x00017b60   0x00000190   Code   RO          736    i.hal_dsi_tx_calc_video_chunks  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017cf0   0x00017cf0   0x00000034   Code   RO          737    i.hal_dsi_tx_config_params_for_lane_rate  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017d24   0x00017d24   0x00000428   Code   RO          738    i.hal_dsi_tx_count_lane_rate  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001814c   0x0001814c   0x0000002c   Code   RO          741    i.hal_dsi_tx_ctrl_create_handle  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018178   0x00018178   0x00000084   Code   RO          742    i.hal_dsi_tx_ctrl_deinit  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000181fc   0x000181fc   0x0000004c   Code   RO          746    i.hal_dsi_tx_ctrl_enter_init_panel_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018248   0x00018248   0x00000028   Code   RO          748    i.hal_dsi_tx_ctrl_exit_init_panel_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018270   0x00018270   0x000000a4   Code   RO          750    i.hal_dsi_tx_ctrl_init  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018314   0x00018314   0x00000024   Code   RO          751    i.hal_dsi_tx_ctrl_init_clk  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018338   0x00018338   0x0000000c   Code   RO          752    i.hal_dsi_tx_ctrl_panel_reset_pin  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018344   0x00018344   0x00000020   Code   RO          755    i.hal_dsi_tx_ctrl_set_ccm  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018364   0x00018364   0x00000014   Code   RO          761    i.hal_dsi_tx_ctrl_set_overwrite_rgb  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018378   0x00018378   0x00000010   Code   RO          762    i.hal_dsi_tx_ctrl_set_partial_disp  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018388   0x00018388   0x00000024   Code   RO          763    i.hal_dsi_tx_ctrl_set_partial_disp_area  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000183ac   0x000183ac   0x000000a8   Code   RO          766    i.hal_dsi_tx_ctrl_start  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018454   0x00018454   0x00000044   Code   RO          767    i.hal_dsi_tx_ctrl_stop  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018498   0x00018498   0x000000cc   Code   RO          769    i.hal_dsi_tx_ctrl_write_cmd  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018564   0x00018564   0x00000044   Code   RO          770    i.hal_dsi_tx_init_data_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000185a8   0x000185a8   0x00000030   Code   RO          771    i.hal_dsi_tx_init_dpi_cfg  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000185d8   0x000185d8   0x00000020   Code   RO          772    i.hal_dsi_tx_init_interrupt  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000185f8   0x000185f8   0x00000020   Code   RO          773    i.hal_dsi_tx_init_phy_cfg  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018618   0x00018618   0x00000094   Code   RO          774    i.hal_dsi_tx_init_remains  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000186ac   0x000186ac   0x00000058   Code   RO          775    i.hal_dsi_tx_init_video_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018704   0x00018704   0x00000044   Code   RO          776    i.hal_dsi_tx_send_cmd  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018748   0x00018748   0x00000018   Code   RO          843    i.hal_gpio_ctrl_eint  CVWL568.lib(hal_gpio.o)
    0x00018760   0x00018760   0x00000012   Code   RO          844    i.hal_gpio_get_input_data  CVWL568.lib(hal_gpio.o)
    0x00018772   0x00018772   0x00000002   PAD
    0x00018774   0x00018774   0x00000040   Code   RO          847    i.hal_gpio_init_eint  CVWL568.lib(hal_gpio.o)
    0x000187b4   0x000187b4   0x00000020   Code   RO          848    i.hal_gpio_init_input  CVWL568.lib(hal_gpio.o)
    0x000187d4   0x000187d4   0x00000028   Code   RO          849    i.hal_gpio_init_output  CVWL568.lib(hal_gpio.o)
    0x000187fc   0x000187fc   0x00000018   Code   RO          850    i.hal_gpio_reg_eint_cb  CVWL568.lib(hal_gpio.o)
    0x00018814   0x00018814   0x00000050   Code   RO          851    i.hal_gpio_set_ap_reset_int  CVWL568.lib(hal_gpio.o)
    0x00018864   0x00018864   0x00000060   Code   RO          853    i.hal_gpio_set_mode  CVWL568.lib(hal_gpio.o)
    0x000188c4   0x000188c4   0x00000008   Code   RO          854    i.hal_gpio_set_output_data  CVWL568.lib(hal_gpio.o)
    0x000188cc   0x000188cc   0x00000020   Code   RO          856    i.hal_gpio_set_pull_state  CVWL568.lib(hal_gpio.o)
    0x000188ec   0x000188ec   0x0000006c   Code   RO          882    i.hal_i2c_m_dma_init  CVWL568.lib(hal_i2c_master.o)
    0x00018958   0x00018958   0x00000020   Code   RO          883    i.hal_i2c_m_dma_read  CVWL568.lib(hal_i2c_master.o)
    0x00018978   0x00018978   0x0000001c   Code   RO          884    i.hal_i2c_m_dma_write  CVWL568.lib(hal_i2c_master.o)
    0x00018994   0x00018994   0x0000000c   Code   RO          886    i.hal_i2c_m_transfer_complate  CVWL568.lib(hal_i2c_master.o)
    0x000189a0   0x000189a0   0x00000020   Code   RO          887    i.hal_i2c_master_irq_callback  CVWL568.lib(hal_i2c_master.o)
    0x000189c0   0x000189c0   0x00000010   Code   RO          901    i.hal_i2c_s_dma_user_callback  CVWL568.lib(hal_i2c_slave.o)
    0x000189d0   0x000189d0   0x0000004c   Code   RO          902    i.hal_i2c_s_dma_write  CVWL568.lib(hal_i2c_slave.o)
    0x00018a1c   0x00018a1c   0x000000c8   Code   RO          904    i.hal_i2c_s_init    CVWL568.lib(hal_i2c_slave.o)
    0x00018ae4   0x00018ae4   0x00000014   Code   RO          905    i.hal_i2c_s_nonblocking_read  CVWL568.lib(hal_i2c_slave.o)
    0x00018af8   0x00018af8   0x0000000c   Code   RO          913    i.hal_i2c_s_set_transfer  CVWL568.lib(hal_i2c_slave.o)
    0x00018b04   0x00018b04   0x00000174   Code   RO          916    i.hal_i2c_slave_irq_callback  CVWL568.lib(hal_i2c_slave.o)
    0x00018c78   0x00018c78   0x00000018   Code   RO         1132    i.hal_internal_check_video_auto_sync  CVWL568.lib(hal_internal_vsync.o)
    0x00018c90   0x00018c90   0x000000fc   Code   RO         1133    i.hal_internal_init_memc  CVWL568.lib(hal_internal_vsync.o)
    0x00018d8c   0x00018d8c   0x0000002a   Code   RO         1134    i.hal_internal_rx_dcs_async_handler  CVWL568.lib(hal_internal_vsync.o)
    0x00018db6   0x00018db6   0x00000002   PAD
    0x00018db8   0x00018db8   0x00000058   Code   RO         1135    i.hal_internal_rx_dcs_polling  CVWL568.lib(hal_internal_vsync.o)
    0x00018e10   0x00018e10   0x00000010   Code   RO         1137    i.hal_internal_sync_get_fb_setting  CVWL568.lib(hal_internal_vsync.o)
    0x00018e20   0x00018e20   0x00000010   Code   RO         1138    i.hal_internal_sync_get_hight_performan_mode  CVWL568.lib(hal_internal_vsync.o)
    0x00018e30   0x00018e30   0x0000022c   Code   RO         1139    i.hal_internal_sync_input_resolution_change  CVWL568.lib(hal_internal_vsync.o)
    0x0001905c   0x0001905c   0x00000028   Code   RO         1142    i.hal_internal_vsync_deinit  CVWL568.lib(hal_internal_vsync.o)
    0x00019084   0x00019084   0x0000000c   Code   RO         1143    i.hal_internal_vsync_get_rx_state  CVWL568.lib(hal_internal_vsync.o)
    0x00019090   0x00019090   0x00000018   Code   RO         1144    i.hal_internal_vsync_get_sync_line  CVWL568.lib(hal_internal_vsync.o)
    0x000190a8   0x000190a8   0x0000000c   Code   RO         1145    i.hal_internal_vsync_get_tear_mode  CVWL568.lib(hal_internal_vsync.o)
    0x000190b4   0x000190b4   0x0000000c   Code   RO         1146    i.hal_internal_vsync_get_tx_state  CVWL568.lib(hal_internal_vsync.o)
    0x000190c0   0x000190c0   0x00000140   Code   RO         1147    i.hal_internal_vsync_init_rx  CVWL568.lib(hal_internal_vsync.o)
    0x00019200   0x00019200   0x000000b0   Code   RO         1148    i.hal_internal_vsync_init_tx  CVWL568.lib(hal_internal_vsync.o)
    0x000192b0   0x000192b0   0x00000090   Code   RO         1150    i.hal_internal_vsync_set_auto_hw_filter  CVWL568.lib(hal_internal_vsync.o)
    0x00019340   0x00019340   0x00000024   Code   RO         1152    i.hal_internal_vsync_set_rx_state  CVWL568.lib(hal_internal_vsync.o)
    0x00019364   0x00019364   0x00000050   Code   RO         1154    i.hal_internal_vsync_set_tear_mode  CVWL568.lib(hal_internal_vsync.o)
    0x000193b4   0x000193b4   0x00000084   Code   RO         1155    i.hal_internal_vsync_set_tx_state  CVWL568.lib(hal_internal_vsync.o)
    0x00019438   0x00019438   0x00000010   Code   RO         1795    i.hal_intl_svs_deinit_tx  CVWL568.lib(hal_internal_soft_sync.o)
    0x00019448   0x00019448   0x00000024   Code   RO         1796    i.hal_intl_svs_handle  CVWL568.lib(hal_internal_soft_sync.o)
    0x0001946c   0x0001946c   0x00000078   Code   RO         1797    i.hal_intl_svs_init_rx  CVWL568.lib(hal_internal_soft_sync.o)
    0x000194e4   0x000194e4   0x00000014   Code   RO         1798    i.hal_intl_svs_init_tx  CVWL568.lib(hal_internal_soft_sync.o)
    0x000194f8   0x000194f8   0x00000048   Code   RO         1801    i.hal_intl_svs_update_rxbr_clk  CVWL568.lib(hal_internal_soft_sync.o)
    0x00019540   0x00019540   0x00000024   Code   RO          777    i.hal_lcdc_config_ccm  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00019564   0x00019564   0x00000064   Code   RO          778    i.hal_lcdc_config_remains  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000195c8   0x000195c8   0x00000014   Code   RO          779    i.hal_lcdc_config_rgb_to_pentile  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000195dc   0x000195dc   0x00000164   Code   RO          780    i.hal_lcdc_config_upscaler  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00019740   0x00019740   0x00000054   Code   RO          781    i.hal_lcdc_init_cfg  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00019794   0x00019794   0x000001cc   Code   RO          782    i.hal_lcdc_init_clk  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00019960   0x00019960   0x00000040   Code   RO          783    i.hal_lcdc_init_interrupt  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000199a0   0x000199a0   0x0000000e   Code   RO          941    i.hal_spi_m_clear_rxfifo  CVWL568.lib(hal_spi_master.o)
    0x000199ae   0x000199ae   0x00000012   Code   RO          965    i.hal_swire_deinit  CVWL568.lib(hal_swire.o)
    0x000199c0   0x000199c0   0x00000016   Code   RO          967    i.hal_swire_open    CVWL568.lib(hal_swire.o)
    0x000199d6   0x000199d6   0x00000008   Code   RO          982    i.hal_system_enable_systick  CVWL568.lib(hal_system.o)
    0x000199de   0x000199de   0x00000002   PAD
    0x000199e0   0x000199e0   0x00000088   Code   RO          986    i.hal_system_init   CVWL568.lib(hal_system.o)
    0x00019a68   0x00019a68   0x0000001c   Code   RO          987    i.hal_system_init_console  CVWL568.lib(hal_system.o)
    0x00019a84   0x00019a84   0x00000008   Code   RO          990    i.hal_system_set_phy_calibration  CVWL568.lib(hal_system.o)
    0x00019a8c   0x00019a8c   0x00000008   Code   RO          991    i.hal_system_set_pvd  CVWL568.lib(hal_system.o)
    0x00019a94   0x00019a94   0x00000008   Code   RO          992    i.hal_system_set_vcc  CVWL568.lib(hal_system.o)
    0x00019a9c   0x00019a9c   0x0000002e   Code   RO         1015    i.hal_timer_deinit  CVWL568.lib(hal_timer.o)
    0x00019aca   0x00019aca   0x0000001a   Code   RO         1017    i.hal_timer_init    CVWL568.lib(hal_timer.o)
    0x00019ae4   0x00019ae4   0x00000048   Code   RO         1019    i.hal_timer_start   CVWL568.lib(hal_timer.o)
    0x00019b2c   0x00019b2c   0x00000028   Code   RO         1021    i.hal_timer_stop    CVWL568.lib(hal_timer.o)
    0x00019b54   0x00019b54   0x00000030   Code   RO          784    i.hal_tx_frame_rate_adjust  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00019b84   0x00019b84   0x0000008c   Code   RO         1107    i.hal_uart_init     CVWL568.lib(hal_uart.o)
    0x00019c10   0x00019c10   0x00000010   Code   RO         1110    i.hal_uart_transmit_blocking  CVWL568.lib(hal_uart.o)
    0x00019c20   0x00019c20   0x00000110   Code   RO         2295    i.handle_init       CVWL568.lib(irq_redirect .o)
    0x00019d30   0x00019d30   0x000000b8   Code   RO          123    i.init_mipi_tx      ap_demo.o
    0x00019de8   0x00019de8   0x00002a56   Code   RO          124    i.init_panel        ap_demo.o
    0x0001c83e   0x0001c83e   0x00000010   Code   RO            3    i.main              main.o
    0x0001c84e   0x0001c84e   0x00000002   PAD
    0x0001c850   0x0001c850   0x00000128   Code   RO          125    i.open_mipi_rx      ap_demo.o
    0x0001c978   0x0001c978   0x00000098   Code   RO          126    i.pps_update_handle  ap_demo.o
    0x0001ca10   0x0001ca10   0x000003f4   Code   RO         1159    i.rx_get_dcs_packet_data  CVWL568.lib(hal_internal_vsync.o)
    0x0001ce04   0x0001ce04   0x0000016c   Code   RO         1160    i.rx_partial_update  CVWL568.lib(hal_internal_vsync.o)
    0x0001cf70   0x0001cf70   0x0000008c   Code   RO         1161    i.rx_receive_packet  CVWL568.lib(hal_internal_vsync.o)
    0x0001cffc   0x0001cffc   0x00000180   Code   RO         1162    i.rx_receive_pps    CVWL568.lib(hal_internal_vsync.o)
    0x0001d17c   0x0001d17c   0x000000cc   Code   RO         1163    i.rxbr_irq0_callback  CVWL568.lib(hal_internal_vsync.o)
    0x0001d248   0x0001d248   0x00000244   Code   RO         1164    i.rxbr_irq1_callback  CVWL568.lib(hal_internal_vsync.o)
    0x0001d48c   0x0001d48c   0x00000034   Code   RO          127    i.set_soft_tear_mode  ap_demo.o
    0x0001d4c0   0x0001d4c0   0x000000c4   Code   RO         1165    i.soft_gen_te       CVWL568.lib(hal_internal_vsync.o)
    0x0001d584   0x0001d584   0x000000c0   Code   RO         1166    i.soft_gen_te_double_buffer  CVWL568.lib(hal_internal_vsync.o)
    0x0001d644   0x0001d644   0x00000038   Code   RO          131    i.soft_te_timer_cb  ap_demo.o
    0x0001d67c   0x0001d67c   0x00000028   Code   RO          132    i.soft_te_timer_init  ap_demo.o
    0x0001d6a4   0x0001d6a4   0x0000003c   Code   RO          133    i.soft_timer3_cb    ap_demo.o
    0x0001d6e0   0x0001d6e0   0x00000048   Code   RO         2758    i.sqrt              m_ps.l(sqrt.o)
    0x0001d728   0x0001d728   0x000000ac   Code   RO         1802    i.svs_direct_mode_setting  CVWL568.lib(hal_internal_soft_sync.o)
    0x0001d7d4   0x0001d7d4   0x0000001c   Code   RO         1803    i.svs_get_rel_intv  CVWL568.lib(hal_internal_soft_sync.o)
    0x0001d7f0   0x0001d7f0   0x000000b0   Code   RO         1804    i.svs_sync_handle   CVWL568.lib(hal_internal_soft_sync.o)
    0x0001d8a0   0x0001d8a0   0x000000f4   Code   RO         1805    i.svs_wait_start    CVWL568.lib(hal_internal_soft_sync.o)
    0x0001d994   0x0001d994   0x000000d8   Code   RO         1806    i.svs_waite_fr_stab  CVWL568.lib(hal_internal_soft_sync.o)
    0x0001da6c   0x0001da6c   0x00000058   Code   RO          137    i.tp_heartbeat_exec  ap_demo.o
    0x0001dac4   0x0001dac4   0x00000030   Code   RO          138    i.tx_display_on     ap_demo.o
    0x0001daf4   0x0001daf4   0x0000006c   Code   RO          139    i.tx_panel_reset    ap_demo.o
    0x0001db60   0x0001db60   0x00000108   Code   RO         1167    i.vidc_callback     CVWL568.lib(hal_internal_vsync.o)
    0x0001dc68   0x0001dc68   0x000000d8   Code   RO         1168    i.vpre_err_reset    CVWL568.lib(hal_internal_vsync.o)
    0x0001dd40   0x0001dd40   0x000001cc   Code   RO         1169    i.vsync_set_te_mode  CVWL568.lib(hal_internal_vsync.o)
    0x0001df0c   0x0001df0c   0x00000178   Data   RO          140    .constdata          ap_demo.o
    0x0001e084   0x0001e084   0x00000020   Data   RO          519    .constdata          app_tp_st_touch.o
    0x0001e0a4   0x0001e0a4   0x00000024   Data   RO          786    .constdata          CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001e0c8   0x0001e0c8   0x000000d2   Data   RO          859    .constdata          CVWL568.lib(hal_gpio.o)
    0x0001e19a   0x0001e19a   0x00000002   PAD
    0x0001e19c   0x0001e19c   0x00000020   Data   RO          917    .constdata          CVWL568.lib(hal_i2c_slave.o)
    0x0001e1bc   0x0001e1bc   0x00000656   Data   RO         1056    .constdata          CVWL568_MI10PRO_HX667_TP.lib(app_tp_for_custom_s8.o)
    0x0001e812   0x0001e812   0x00000002   PAD
    0x0001e814   0x0001e814   0x00000008   Data   RO         1622    .constdata          CVWL568.lib(drv_param_init.o)
    0x0001e81c   0x0001e81c   0x00000186   Data   RO         2367    .constdata          CVWL568.lib(drv_phy_common.o)
    0x0001e9a2   0x0001e9a2   0x00000002   PAD
    0x0001e9a4   0x0001e9a4   0x00000050   Data   RO          141    .conststring        ap_demo.o
    0x0001e9f4   0x0001e9f4   0x00000048   Data   RO          683    .conststring        CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001ea3c   0x0001ea3c   0x00000043   Data   RO          787    .conststring        CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001ea7f   0x0001ea7f   0x00000001   PAD
    0x0001ea80   0x0001ea80   0x00000178   Data   RO         1171    .conststring        CVWL568.lib(hal_internal_vsync.o)
    0x0001ebf8   0x0001ebf8   0x00000030   Data   RO         3122    Region$$Table       anon$$obj.o


    Execution Region RW_RAM1 (Exec base: 0x00070000, Load base: 0x0001ec28, Size: 0x00000000, Max: 0x000000f0, ABSOLUTE)

    **** No section assigned to this execution region ****


    Execution Region RW_RAM2 (Exec base: 0x00070100, Load base: 0x0001ec28, Size: 0x000000c0, Max: 0x000000d0, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00070100        -       0x000000c0   Zero   RW         2296    .ARM.__AT_0x00070100  CVWL568.lib(irq_redirect .o)


    Execution Region RW_RAM3 (Exec base: 0x000701d0, Load base: 0x0001ec28, Size: 0x00003c60, Max: 0x00007e30, ABSOLUTE, COMPRESSED[0x000006b4])

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x000701d0   COMPRESSED   0x00000248   Data   RW          142    .data               ap_demo.o
    0x00070418   COMPRESSED   0x00000040   Data   RW          377    .data               app_tp_transfer.o
    0x00070458   COMPRESSED   0x00000028   Data   RW          520    .data               app_tp_st_touch.o
    0x00070480   COMPRESSED   0x00000008   Data   RW          684    .data               CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00070488   COMPRESSED   0x00000003   Data   RW          788    .data               CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0007048b   COMPRESSED   0x00000001   Data   RW          888    .data               CVWL568.lib(hal_i2c_master.o)
    0x0007048c   COMPRESSED   0x00000020   Data   RW          918    .data               CVWL568.lib(hal_i2c_slave.o)
    0x000704ac   COMPRESSED   0x0000031a   Data   RW         1057    .data               CVWL568_MI10PRO_HX667_TP.lib(app_tp_for_custom_s8.o)
    0x000707c6   COMPRESSED   0x00000002   PAD
    0x000707c8   COMPRESSED   0x00000018   Data   RW         1172    .data               CVWL568.lib(hal_internal_vsync.o)
    0x000707e0   COMPRESSED   0x0000000c   Data   RW         1233    .data               CVWL568.lib(drv_common.o)
    0x000707ec   COMPRESSED   0x00000004   Data   RW         1500    .data               CVWL568.lib(drv_gpio.o)
    0x000707f0   COMPRESSED   0x00000008   Data   RW         1538    .data               CVWL568.lib(drv_i2c_dma.o)
    0x000707f8   COMPRESSED   0x00000004   Data   RW         1567    .data               CVWL568.lib(drv_i2c_master.o)
    0x000707fc   COMPRESSED   0x00000004   Data   RW         1598    .data               CVWL568.lib(drv_i2c_slave.o)
    0x00070800   COMPRESSED   0x000004a4   Data   RW         1623    .data               CVWL568.lib(drv_param_init.o)
    0x00070ca4   COMPRESSED   0x00000004   Data   RW         1690    .data               CVWL568.lib(drv_spi_master.o)
    0x00070ca8   COMPRESSED   0x00000008   Data   RW         1716    .data               CVWL568.lib(drv_swire.o)
    0x00070cb0   COMPRESSED   0x00000001   Data   RW         1741    .data               CVWL568.lib(drv_sys_cfg.o)
    0x00070cb1   COMPRESSED   0x00000003   PAD
    0x00070cb4   COMPRESSED   0x00000050   Data   RW         1774    .data               CVWL568.lib(drv_timer.o)
    0x00070d04   COMPRESSED   0x00000008   Data   RW         2145    .data               CVWL568.lib(drv_rxbr.o)
    0x00070d0c   COMPRESSED   0x00000004   Data   RW         2221    .data               CVWL568.lib(drv_vidc.o)
    0x00070d10   COMPRESSED   0x00000001   Data   RW         2368    .data               CVWL568.lib(drv_phy_common.o)
    0x00070d11   COMPRESSED   0x00000003   PAD
    0x00070d14   COMPRESSED   0x0000000c   Data   RW         2388    .data               CVWL568.lib(drv_chip_info.o)
    0x00070d20   COMPRESSED   0x00000012   Data   RW         2497    .data               CVWL568.lib(norflash.o)
    0x00070d32   COMPRESSED   0x00000002   PAD
    0x00070d34   COMPRESSED   0x0000000c   Data   RW         2584    .data               CVWL568.lib(drv_pwm.o)
    0x00070d40   COMPRESSED   0x00000008   Data   RW         2662    .data               CVWL568.lib(drv_uart.o)
    0x00070d48   COMPRESSED   0x0000000c   Data   RW         2729    .data               CVWL568.lib(drv_wdg.o)
    0x00070d54   COMPRESSED   0x00000004   Data   RW         3091    .data               mc_p.l(stdout.o)
    0x00070d58   COMPRESSED   0x00000004   Data   RW         3103    .data               mc_p.l(errno.o)
    0x00070d5c        -       0x00000244   Zero   RW          376    .bss                app_tp_transfer.o
    0x00070fa0        -       0x0000000c   Zero   RW          518    .bss                app_tp_st_touch.o
    0x00070fac        -       0x000000c4   Zero   RW          682    .bss                CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00071070        -       0x0000004c   Zero   RW          785    .bss                CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000710bc        -       0x00000100   Zero   RW         1044    .bss                CVWL568.lib(tau_log.o)
    0x000711bc        -       0x000000d0   Zero   RW         1112    .bss                CVWL568.lib(hal_uart.o)
    0x0007128c        -       0x00000974   Zero   RW         1170    .bss                CVWL568.lib(hal_internal_vsync.o)
    0x00071c00        -       0x0000001c   Zero   RW         1362    .bss                CVWL568.lib(drv_dma.o)
    0x00071c1c        -       0x00000040   Zero   RW         1499    .bss                CVWL568.lib(drv_gpio.o)
    0x00071c5c        -       0x00000140   Zero   RW         1537    .bss                CVWL568.lib(drv_i2c_dma.o)
    0x00071d9c        -       0x00000040   Zero   RW         1807    .bss                CVWL568.lib(hal_internal_soft_sync.o)
    0x00071ddc        -       0x00000020   Zero   RW         2432    .bss                CVWL568.lib(hal_spi_slave.o)
    0x00071dfc        -       0x00001030   Zero   RW         2747    .bss                CVWL568.lib(dcs_packet_fifo.o)
    0x00072e2c   COMPRESSED   0x00000004   PAD
    0x00072e30        -       0x00001000   Zero   RW          629    STACK               startup_armcm0.o


==============================================================================

Image component sizes


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Object Name

     14752        890        456        584          0      30323   ap_demo.o
      1546        288         32         40         12      11229   app_tp_st_touch.o
      1138        132          0         64        580      13001   app_tp_transfer.o
        36          6          0          0          0        485   board.o
        16          0          0          0          0       9591   main.o
       120         18        192          0       4096       2068   startup_armcm0.o

    ----------------------------------------------------------------------
     17618       1334        728        688       4688      66697   Object Totals
         0          0         48          0          0          0   (incl. Generated)
        10          0          0          0          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Member Name

       216         32          0          0       4144        252   dcs_packet_fifo.o
       272         96          0         12          0        256   drv_chip_info.o
       192         82         24         12          0        264   drv_common.o
       420         90          0          0          0       1200   drv_crgu.o
       410         28          0          0         28        796   drv_dma.o
       232         28          0          0          0        340   drv_dsc_dec.o
      1658        494          0          0          0       1396   drv_dsi_rx.o
      1528        118          0          0          0       2428   drv_dsi_tx.o
       132          0          0          0          0        256   drv_efuse.o
        10          0          0          0          0         60   drv_fls.o
       796        112          0          4         64       1236   drv_gpio.o
       600         82          0          8        320        624   drv_i2c_dma.o
       360         86          0          4          0        456   drv_i2c_master.o
       292         36          0          4          0        580   drv_i2c_slave.o
       704          6          0          0          0       1504   drv_lcdc.o
       492         28          0          0          0       1112   drv_memc.o
       212         44          8       1188          0        452   drv_param_init.o
       428         30        390          1          0        664   drv_phy_common.o
        72         10          0         12          0         76   drv_pwm.o
       112         24          0          0          0        180   drv_pwr.o
       548         74          0          8          0       1500   drv_rxbr.o
       104         24          0          4          0        188   drv_spi_master.o
       172         20          0          8          0        260   drv_swire.o
       300         64          0          1          0        628   drv_sys_cfg.o
       374         34          0         80          0        932   drv_timer.o
       698         18          0          8          0        680   drv_uart.o
       510         28          0          4          0       1452   drv_vidc.o
       168         22          0         12          0        316   drv_wdg.o
      3342        324         72          8        196       1760   hal_dsi_rx_ctrl.o
      4216        310        103          3         76       2400   hal_dsi_tx_ctrl.o
       450         48        210          0          0        752   hal_gpio.o
       212         40          0          1          0        340   hal_i2c_master.o
       696         70         32         32          0        408   hal_i2c_slave.o
      1100        184          0          0         64        716   hal_internal_soft_sync.o
      7996       1624        376         24       2420       2668   hal_internal_vsync.o
        14          0          0          0          0         68   hal_spi_master.o
       580         32          0          0         32        136   hal_spi_slave.o
        40          0          0          0          0        136   hal_swire.o
       196         32          0          0          0        408   hal_system.o
       184          6          0          0          0        276   hal_timer.o
       156         18          0          0        208        144   hal_uart.o
      1076        324          0          0        192       1980   irq_redirect .o
        48         10          0         18          0         68   norflash.o
        58          0          0          0          0        128   tau_delay.o
        60         10          0          0        256        156   tau_log.o
      1376        148       1622        794          0      15398   app_tp_for_custom_s8.o
       200         20          0          0          0         76   ceil.o
        72          6          0          0          0         76   sqrt.o
        86          0          0          0          0          0   __dczerorl2.o
         0          0          0          0          0          0   entry.o
         0          0          0          0          0          0   entry10a.o
         0          0          0          0          0          0   entry11a.o
         8          4          0          0          0          0   entry2.o
         4          0          0          0          0          0   entry5.o
         0          0          0          0          0          0   entry7b.o
         0          0          0          0          0          0   entry8b.o
         8          4          0          0          0          0   entry9a.o
        12          6          0          4          0         60   errno.o
        30          0          0          0          0          0   handlers.o
        40          0          0          0          0         72   idiv.o
        36          8          0          0          0         68   init.o
         0          0          0          0          0          0   iusefp.o
        32          0          0          0          0         68   llshl.o
        38          0          0          0          0         68   llsshr.o
        34          0          0          0          0         68   llushr.o
        36          0          0          0          0         60   memcpya.o
        36          0          0          0          0        100   memseta.o
      2298        104          0          0          0        544   printfa.o
         0          0          0          4          0          0   stdout.o
        44          0          0          0          0         72   uidiv.o
        96          0          0          0          0         84   uldiv.o
        40          2          0          0          0         68   cdcmple.o
        40          2          0          0          0         68   cdrcmple.o
        20          0          0          0          0         68   cfcmple.o
        20          0          0          0          0         68   cfrcmple.o
       356          4          0          0          0        140   dadd.o
       240          6          0          0          0         84   ddiv.o
       236          0          0          0          0        216   depilogue.o
        72         10          0          0          0         72   dfixi.o
        60         10          0          0          0         68   dfixui.o
        64         10          0          0          0         68   dfixul.o
        28          4          0          0          0         68   dfltui.o
       208          6          0          0          0         88   dmul.o
       162          0          0          0          0         80   dsqrt.o
        40          0          0          0          0         60   f2d.o
       178          0          0          0          0        108   fadd.o
       124          0          0          0          0         72   fdiv.o
       130          0          0          0          0        144   fepilogue.o
        50          0          0          0          0         60   ffixi.o
        40          0          0          0          0         60   ffixui.o
        22          0          0          0          0         68   fflti.o
        14          0          0          0          0         68   ffltui.o
       122          0          0          0          0         72   fmul.o
        24          0          0          0          0         60   fscalb.o

    ----------------------------------------------------------------------
     39266       5096       2844       2268       8004      51374   Library Totals
        54          0          7         10          4          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Name

     32436       4742       1215       1456       8000      32632   CVWL568.lib
      1376        148       1622        794          0      15398   CVWL568_MI10PRO_HX667_TP.lib
       272         26          0          0          0        152   m_ps.l
      2838        126          0          8          0       1264   mc_p.l
      2290         54          0          0          0       1928   mf_p.l

    ----------------------------------------------------------------------
     39266       5096       2844       2268       8004      51374   Library Totals

    ----------------------------------------------------------------------

==============================================================================


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   

     56884       6430       3572       2956      12692      92391   Grand Totals
     56884       6430       3572       1716      12692      92391   ELF Image Totals (compressed)
     56884       6430       3572       1716          0          0   ROM Totals

==============================================================================

    Total RO  Size (Code + RO Data)                60456 (  59.04kB)
    Total RW  Size (RW Data + ZI Data)             15648 (  15.28kB)
    Total ROM Size (Code + RO Data + RW Data)      62172 (  60.71kB)

==============================================================================

