Component: ARM Compiler 5.06 update 6 (build 750) Tool: armlink [4d35ed]

==============================================================================

Section Cross References

    main.o(i.main) refers to board.o(i.board_Init) for board_Init
    main.o(i.main) refers to ap_demo.o(i.ap_demo) for ap_demo
    ap_demo.o(i.Gpio_swire_output) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    ap_demo.o(i.Gpio_swire_output) refers to tau_delay.o(i.delayUs) for delayUs
    ap_demo.o(i.Gpio_swire_output) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    ap_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) for hal_dsi_rx_ctrl_get_max_ret_size
    ap_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) for hal_dsi_rx_ctrl_send_ack_cmd
    ap_demo.o(i.ap_dcs_read) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_dcs_read) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_demo) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_I2C_init) for app_tp_I2C_init
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.open_mipi_rx) for open_mipi_rx
    ap_demo.o(i.ap_demo) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.init_mipi_tx) for init_mipi_tx
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_init) for app_tp_init
    ap_demo.o(i.ap_demo) refers to hal_timer.o(i.hal_timer_init) for hal_timer_init
    ap_demo.o(i.ap_demo) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.tx_display_on) for tx_display_on
    ap_demo.o(i.ap_demo) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_phone_clear_reset_on) for app_tp_phone_clear_reset_on
    ap_demo.o(i.ap_demo) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_transfer_screen_start) for app_tp_transfer_screen_start
    ap_demo.o(i.ap_demo) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) for hal_dsi_rx_ctrl_dsc_async_handler
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.app_tp_calibration_exec) for app_tp_calibration_exec
    ap_demo.o(i.ap_demo) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_demo) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_transfer_screen_int) for app_tp_transfer_screen_int
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.tp_heartbeat_exec) for tp_heartbeat_exec
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.ap_tp_scan_point_record_event_exec) for ap_tp_scan_point_record_event_exec
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.S20_Start_init) for S20_Start_init
    ap_demo.o(i.ap_demo) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_demo) refers to app_tp_for_custom_s8.o(.data) for tp_sleep_count
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.soft_timer3_cb) for soft_timer3_cb
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.ap_reset_cb) for ap_reset_cb
    ap_demo.o(i.ap_get_reg_ca) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_get_reg_df) refers to ap_demo.o(i.blue_change_ccm) for blue_change_ccm
    ap_demo.o(i.ap_get_reg_df) refers to memcpya.o(.text) for __aeabi_memcpy4
    ap_demo.o(i.ap_get_reg_df) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) for hal_dsi_tx_ctrl_set_ccm
    ap_demo.o(i.ap_get_reg_df) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_reset_cb) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_reset_cb) refers to hal_system.o(i.hal_system_set_pvd) for hal_system_set_pvd
    ap_demo.o(i.ap_reset_cb) refers to hal_system.o(i.hal_system_set_vcc) for hal_system_set_vcc
    ap_demo.o(i.ap_set_backlight) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    ap_demo.o(i.ap_set_backlight) refers to idiv.o(.text) for __aeabi_idivmod
    ap_demo.o(i.ap_set_backlight) refers to uidiv.o(.text) for __aeabi_uidivmod
    ap_demo.o(i.ap_set_backlight) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_backlight) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_set_display_off) refers to ap_demo.o(i.Gpio_swire_output) for Gpio_swire_output
    ap_demo.o(i.ap_set_display_off) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_display_off) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_display_off) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_set_display_on) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_display_on) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to ap_demo.o(i.soft_disable_mipi_timer_init) for soft_disable_mipi_timer_init
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_set_exit_sleep_mode) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_exit_sleep_mode) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_set_tp_calibration_04) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.app_tp_calibration_exec) refers to app_tp_transfer.o(i.ap_tp_calibration) for ap_tp_calibration
    ap_demo.o(i.app_tp_calibration_exec) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.app_tp_calibration_exec) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.blue_change_ccm) refers to memcpya.o(.text) for __aeabi_memcpy4
    ap_demo.o(i.blue_change_ccm) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) for hal_dsi_tx_ctrl_set_ccm
    ap_demo.o(i.disable_mipi_timer_cb) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    ap_demo.o(i.disable_mipi_timer_cb) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) for hal_dsi_tx_ctrl_stop
    ap_demo.o(i.disable_mipi_timer_cb) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) for hal_dsi_tx_ctrl_deinit
    ap_demo.o(i.disable_mipi_timer_cb) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) for hal_dsi_rx_ctrl_stop
    ap_demo.o(i.disable_mipi_timer_cb) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) for hal_dsi_rx_ctrl_deinit
    ap_demo.o(i.disable_mipi_timer_cb) refers to hal_swire.o(i.hal_swire_open) for hal_swire_open
    ap_demo.o(i.disable_mipi_timer_cb) refers to hal_timer.o(i.hal_timer_stop) for hal_timer_stop
    ap_demo.o(i.disable_mipi_timer_cb) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    ap_demo.o(i.disable_mipi_timer_cb) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin) for hal_dsi_tx_ctrl_panel_reset_pin
    ap_demo.o(i.disable_mipi_timer_cb) refers to hal_system.o(i.hal_system_set_vcc) for hal_system_set_vcc
    ap_demo.o(i.disable_mipi_timer_cb) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.disable_mipi_timer_cb) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.disable_mipi_timer_cb) refers to app_tp_for_custom_s8.o(.data) for tp_sleep_in
    ap_demo.o(i.init_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) for hal_dsi_tx_ctrl_create_handle
    ap_demo.o(i.init_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    ap_demo.o(i.init_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) for hal_dsi_tx_ctrl_set_overwrite_rgb
    ap_demo.o(i.init_mipi_tx) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.init_panel) refers to ap_demo.o(i.tx_panel_reset) for tx_panel_reset
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) for hal_dsi_tx_ctrl_enter_init_panel_mode
    ap_demo.o(i.init_panel) refers to ap_demo.o(i.send_panel_init_code) for send_panel_init_code
    ap_demo.o(i.init_panel) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.init_panel) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) for hal_dsi_rx_ctrl_set_hw_tear_mode
    ap_demo.o(i.init_panel) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    ap_demo.o(i.init_panel) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.init_panel) refers to ap_demo.o(i.Gpio_swire_output) for Gpio_swire_output
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) for hal_dsi_tx_ctrl_exit_init_panel_mode
    ap_demo.o(i.init_panel) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.open_mipi_rx) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) for hal_dsi_rx_ctrl_create_handle
    ap_demo.o(i.open_mipi_rx) refers to memcpya.o(.text) for __aeabi_memcpy4
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) for hal_dsi_rx_ctrl_pre_init_pps
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) for hal_dsi_rx_ctrl_set_cus_sync_line
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(.constdata) for .constdata
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(i.ap_dcs_read) for ap_dcs_read
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(i.pps_update_handle) for pps_update_handle
    ap_demo.o(i.pps_update_handle) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) for hal_dsi_rx_ctrl_set_sw_tear_mode
    ap_demo.o(i.pps_update_handle) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) for hal_dsi_rx_ctrl_toggle_resolution
    ap_demo.o(i.pps_update_handle) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) for hal_dsi_rx_ctrl_set_hw_tear_mode
    ap_demo.o(i.pps_update_handle) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.send_panel_init_code) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) for hal_dsi_tx_ctrl_write_array_cmd
    ap_demo.o(i.send_panel_init_code) refers to tau_delay.o(i.delayUs) for delayUs
    ap_demo.o(i.soft_disable_mipi_timer_init) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.soft_disable_mipi_timer_init) refers to hal_timer.o(i.hal_timer_init) for hal_timer_init
    ap_demo.o(i.soft_disable_mipi_timer_init) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    ap_demo.o(i.soft_disable_mipi_timer_init) refers to ap_demo.o(i.disable_mipi_timer_cb) for disable_mipi_timer_cb
    ap_demo.o(i.soft_timer3_cb) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    ap_demo.o(i.soft_timer3_cb) refers to app_tp_for_custom_s8.o(.data) for tp_sleep_count
    ap_demo.o(i.soft_timer3_cb) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.tp_heartbeat_exec) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    ap_demo.o(i.tp_heartbeat_exec) refers to printfa.o(i.__0printf) for __2printf
    ap_demo.o(i.tp_heartbeat_exec) refers to app_tp_transfer.o(i.ap_tp_system_softReset) for ap_tp_system_softReset
    ap_demo.o(i.tp_heartbeat_exec) refers to app_tp_transfer.o(.data) for s_screen_init_complate
    ap_demo.o(i.tp_heartbeat_exec) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.tx_display_on) refers to ap_demo.o(i.init_panel) for init_panel
    ap_demo.o(i.tx_display_on) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    ap_demo.o(i.tx_display_on) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.tx_panel_reset) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin) for hal_dsi_tx_ctrl_panel_reset_pin
    ap_demo.o(i.tx_panel_reset) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_display_on) for ap_set_display_on
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_display_off) for ap_set_display_off
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_get_reg_df) for ap_get_reg_df
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_get_reg_ca) for ap_get_reg_ca
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_backlight) for ap_set_backlight
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_enter_sleep_mode) for ap_set_enter_sleep_mode
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_exit_sleep_mode) for ap_set_exit_sleep_mode
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_tp_calibration_04) for ap_set_tp_calibration_04
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to app_tp_for_custom_s8.o(.data) for .data
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to app_tp_for_custom_s8.o(.constdata) for .constdata
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to app_tp_transfer.o(i.app_tp_screen_init) for app_tp_screen_init
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to app_tp_for_custom_s8.o(.data) for .data
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to uidiv.o(.text) for __aeabi_uidivmod
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to app_tp_for_custom_s8.o(.data) for .data
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_1
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_2
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_3
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_4
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_5
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_6
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_7
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_point_data
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_point_back
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_coord_data
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_coord_back
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_transfer.o(i.S20_Start_init) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.S20_Start_init) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(i.app_tp_screen_int_init) for app_tp_screen_int_init
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_for_custom_s8.o(.data) for screen_reg_int_data
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.S20_Start_init) refers to ap_demo.o(.data) for phone_start_flag
    app_tp_transfer.o(i.ap_tp_calibration) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_transfer.o(i.ap_tp_calibration) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.ap_tp_calibration) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_transfer.o(i.ap_tp_calibration) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.ap_tp_scan_point_init) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.ap_tp_scan_point_record_event) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.ap_tp_scan_point_record_event_exec) refers to printfa.o(i.__0printf) for __2printf
    app_tp_transfer.o(i.ap_tp_scan_point_record_event_exec) refers to app_tp_transfer.o(i.ap_tp_simulate_finger_release_event) for ap_tp_simulate_finger_release_event
    app_tp_transfer.o(i.ap_tp_scan_point_record_event_exec) refers to app_tp_transfer.o(i.ap_tp_scan_point_init) for ap_tp_scan_point_init
    app_tp_transfer.o(i.ap_tp_scan_point_record_event_exec) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.ap_tp_simulate_finger_release_event) refers to app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) for app_tp_screen_analysis_int
    app_tp_transfer.o(i.ap_tp_simulate_finger_release_event) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_transfer.o(i.ap_tp_system_softReset) refers to app_tp_transfer.o(i.ap_tp_simulate_finger_release_event) for ap_tp_simulate_finger_release_event
    app_tp_transfer.o(i.ap_tp_system_softReset) refers to app_tp_transfer.o(i.ap_tp_scan_point_init) for ap_tp_scan_point_init
    app_tp_transfer.o(i.ap_tp_system_softReset) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_transfer.o(i.ap_tp_system_softReset) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.ap_tp_system_softReset) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_transfer.o(i.ap_tp_system_softReset) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_I2C_init) refers to hal_i2c_slave.o(i.hal_i2c_s_init) for hal_i2c_s_init
    app_tp_transfer.o(i.app_tp_I2C_init) refers to hal_i2c_slave.o(i.hal_i2c_s_set_transfer) for hal_i2c_s_set_transfer
    app_tp_transfer.o(i.app_tp_I2C_init) refers to hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read) for hal_i2c_s_nonblocking_read
    app_tp_transfer.o(i.app_tp_I2C_init) refers to app_tp_transfer.o(i.app_tp_i2cs_callback) for app_tp_i2cs_callback
    app_tp_transfer.o(i.app_tp_I2C_init) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(i.app_tp_transfer_phone) for app_tp_transfer_phone
    app_tp_transfer.o(i.app_tp_init) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(i.app_tp_screen_init) for app_tp_screen_init
    app_tp_transfer.o(i.app_tp_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    app_tp_transfer.o(i.app_tp_init) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_master.o(i.hal_i2c_m_dma_init) for hal_i2c_m_dma_init
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(i.ap_tp_scan_point_init) for ap_tp_scan_point_init
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_for_custom_s8.o(.data) for g_phone_output_int_pad
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.app_tp_m_read) refers to hal_i2c_master.o(i.hal_i2c_m_dma_read) for hal_i2c_m_dma_read
    app_tp_transfer.o(i.app_tp_m_transfer_complate) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.app_tp_m_write) refers to hal_i2c_master.o(i.hal_i2c_m_dma_write) for hal_i2c_m_dma_write
    app_tp_transfer.o(i.app_tp_phone_clear_reset_on) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_phone_reset_on) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_s_read) refers to hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read) for hal_i2c_s_nonblocking_read
    app_tp_transfer.o(i.app_tp_s_transfer_complate) refers to hal_i2c_slave.o(i.hal_i2c_s_write_complate) for hal_i2c_s_write_complate
    app_tp_transfer.o(i.app_tp_s_transfer_complate) refers to hal_i2c_slave.o(i.hal_i2c_s_read_complate) for hal_i2c_s_read_complate
    app_tp_transfer.o(i.app_tp_s_write) refers to hal_i2c_slave.o(i.hal_i2c_s_dma_write) for hal_i2c_s_dma_write
    app_tp_transfer.o(i.app_tp_screen_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    app_tp_transfer.o(i.app_tp_screen_init) refers to tau_delay.o(i.delayUs) for delayUs
    app_tp_transfer.o(i.app_tp_screen_init) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_transfer.o(i.app_tp_screen_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_rst_pad
    app_tp_transfer.o(i.app_tp_screen_int_callback) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to hal_gpio.o(i.hal_gpio_ctrl_eint) for hal_gpio_ctrl_eint
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to hal_gpio.o(i.hal_gpio_init_eint) for hal_gpio_init_eint
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to hal_gpio.o(i.hal_gpio_reg_eint_cb) for hal_gpio_reg_eint_cb
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to app_tp_transfer.o(i.app_tp_screen_int_callback) for app_tp_screen_int_callback
    app_tp_transfer.o(i.app_tp_transfer_phone) refers to app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) for app_tp_phone_analysis_data
    app_tp_transfer.o(i.app_tp_transfer_phone) refers to app_tp_transfer.o(i.app_tp_s_read) for app_tp_s_read
    app_tp_transfer.o(i.app_tp_transfer_phone) refers to app_tp_transfer.o(i.app_tp_s_write) for app_tp_s_write
    app_tp_transfer.o(i.app_tp_transfer_phone) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(i.app_tp_m_transfer_complate) for app_tp_m_transfer_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to hal_spi_master.o(i.hal_spi_m_clear_rxfifo) for hal_spi_m_clear_rxfifo
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(i.S20_Start_init) for S20_Start_init
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_for_custom_s8.o(.constdata) for screen_reg_start_data_size
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to ap_demo.o(.data) for phone_start_flag
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_transfer_screen_const) for app_tp_transfer_screen_const
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_screen_int_lvl_low) for app_tp_screen_int_lvl_low
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_m_transfer_complate) for app_tp_m_transfer_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_spi_master.o(i.hal_spi_m_clear_rxfifo) for hal_spi_m_clear_rxfifo
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to tau_delay.o(i.delayUs) for delayUs
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.ap_tp_system_softReset) for ap_tp_system_softReset
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to tau_log.o(i.LOG_printf) for LOG_printf
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.ap_tp_scan_point_record_event) for ap_tp_scan_point_record_event
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) for app_tp_screen_analysis_int
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(.data) for screen_reg_int_data
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.app_tp_transfer_screen_start) refers to app_tp_transfer.o(i.app_tp_transfer_screen_const) for app_tp_transfer_screen_const
    app_tp_transfer.o(i.app_tp_transfer_screen_start) refers to app_tp_transfer.o(.data) for .data
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_init) for hal_system_init
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_enable_systick) for hal_system_enable_systick
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_init_console) for hal_system_init_console
    startup_armcm0.o(RESET) refers to startup_armcm0.o(STACK) for __initial_sp
    startup_armcm0.o(RESET) refers to startup_armcm0.o(.text) for Reset_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.HardFault_Handler) for HardFault_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SysTick_Handler) for SysTick_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.VIDC_IRQn_Handler) for VIDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.LCDC_IRQn_Handler) for LCDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.MIPI_RX_IRQn_Handler) for MIPI_RX_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.MIPI_TX_IRQn_Handler) for MIPI_TX_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.MEMC_IRQn_Handler) for MEMC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.VPRE_IRQn_Handler) for VPRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.FLSCTRL_IRQn_Handler) for FLSCTRL_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.DMA_IRQn_Handler) for DMA_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER0_IRQn_Handler) for TIMER0_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER1_IRQn_Handler) for TIMER1_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER2_IRQn_Handler) for TIMER2_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER3_IRQn_Handler) for TIMER3_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.WDG_IRQn_Handler) for WDG_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.UART_IRQn_Handler) for UART_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.I2C0_IRQn_Handler) for I2C0_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.I2C1_IRQn_Handler) for I2C1_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SPIS_IRQn_Handler) for SPIS_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SPIM_IRQn_Handler) for SPIM_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.ADC_IRQn_Handler) for ADC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.PWMDET_IRQn_Handler) for PWMDET_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SWIRE_IRQn_Handler) for SWIRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.AP_NRESET_IRQn_Handler) for AP_NRESET_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT0_IRQn_Handler) for EXTI_INT0_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT1_IRQn_Handler) for EXTI_INT1_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT2_IRQn_Handler) for EXTI_INT2_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT3_IRQn_Handler) for EXTI_INT3_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT4_IRQn_Handler) for EXTI_INT4_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT5_IRQn_Handler) for EXTI_INT5_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT6_IRQn_Handler) for EXTI_INT6_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT7_IRQn_Handler) for EXTI_INT7_IRQn_Handler
    startup_armcm0.o(.text) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) for hal_internal_vsync_get_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) for dcs_packet_get_fifo_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) for dcs_packet_free_fifo_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to hal_dsi_rx_ctrl.o(i.drv_rxbr_get_status) for drv_rxbr_get_status
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg) for drv_dsi_rx_set_ddi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_crgu.o(i.drv_crgu_set_rxbr_src) for drv_crgu_set_rxbr_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_crgu.o(i.drv_crgu_set_rxbr_div) for drv_crgu_set_rxbr_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg) for drv_dsi_rx_set_ipi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_gen_a_tear_signal) for drv_memc_gen_a_tear_signal
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size) for drv_dsi_rx_get_max_ret_size
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_rxbr_src) for drv_crgu_set_rxbr_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_rxbr_div) for drv_crgu_set_rxbr_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_dsco_src) for drv_crgu_set_dsco_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_dsco_src_div) for drv_crgu_set_dsco_src_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_dsc_core_div) for drv_crgu_set_dsc_core_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_vidc_src) for drv_crgu_set_vidc_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_fb_src) for drv_crgu_set_fb_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_fb_div) for drv_crgu_set_fb_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) for hal_dsi_rx_ctrl_init_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_rx) for hal_internal_vsync_init_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) for hal_dsi_rx_ctrl_init_dsi_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) for hal_dsi_rx_ctrl_init_rxbr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsc_dec) for hal_dsi_rx_ctrl_init_dsc_dec
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) for hal_dsi_rx_ctrl_init_vidc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) for hal_dsi_rx_ctrl_init_memc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_chip_info.o(i.drv_chip_rx_init_done) for drv_chip_rx_init_done
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_vidc_src) for drv_crgu_set_vidc_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_fb_src) for drv_crgu_set_fb_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_fb_div) for drv_crgu_set_fb_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) for hal_dsi_rx_ctrl_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsc_dec) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsc_dec) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsc_dec) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps) for drv_dsc_dec_set_u8_pps
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg) for drv_dsi_rx_set_ctrl_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) for drv_dsi_rx_set_up_phy
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_inten) for drv_dsi_rx_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt) for drv_dsi_rx_set_resp_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_hwclr) for drv_memc_set_tear_hwclr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_yuv420_cfg) for drv_memc_set_yuv420_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_bypass_fifo_empty) for drv_memc_bypass_fifo_empty
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_color_format) for drv_rxbr_set_color_format
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_cfg) for drv_rxbr_set_usr_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_col) for drv_rxbr_set_usr_col
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_row) for drv_rxbr_set_usr_row
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg) for drv_rxbr_hline_rcv_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) for hal_internal_vsync_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_src_parameter) for drv_vidc_set_src_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_dst_parameter) for drv_vidc_set_dst_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_module_enable) for drv_vidc_module_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_init_get_scld_filter_h) for drv_param_init_get_scld_filter_h
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_init_get_scld_filter_v) for drv_param_init_get_scld_filter_v
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef0) for drv_vidc_set_scld_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef1) for drv_vidc_set_scld_hcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef0) for drv_vidc_set_scld_vcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef1) for drv_vidc_set_scld_vcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_yuv420_filter_init) for drv_param_yuv420_filter_init
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_y4t2_hcoef0) for drv_vidc_set_y4t2_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_y4t2_hcoef1) for drv_vidc_set_y4t2_hcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_y4t2_vcoef0) for drv_vidc_set_y4t2_vcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_y4t2_vcoef1) for drv_vidc_set_y4t2_vcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_p2r_filter_init) for drv_param_p2r_filter_init
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_p2r_step) for drv_vidc_set_p2r_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_p2r_hinitr) for drv_vidc_set_p2r_hinitr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_p2r_hinitb) for drv_vidc_set_p2r_hinitb
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_p2r_hcoef0) for drv_vidc_set_p2r_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_p2r_hcoef1) for drv_vidc_set_p2r_hcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pu_scld) for drv_vidc_set_pu_scld
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_init_get_sclu_filter_h) for drv_param_init_get_sclu_filter_h
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_init_get_sclu_filter_v) for drv_param_init_get_sclu_filter_v
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_sclu_hcoef0y) for drv_vidc_set_sclu_hcoef0y
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_sclu_hcoef1y) for drv_vidc_set_sclu_hcoef1y
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_sclu_vcoef0y) for drv_vidc_set_sclu_vcoef0y
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_sclu_vcoef1y) for drv_vidc_set_sclu_vcoef1y
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_sclu_hcoef0c) for drv_vidc_set_sclu_hcoef0c
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_sclu_hcoef1c) for drv_vidc_set_sclu_hcoef1c
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_sclu_vcoef0c) for drv_vidc_set_sclu_vcoef0c
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_sclu_vcoef1c) for drv_vidc_set_sclu_vcoef1c
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pu_ctrl) for drv_vidc_set_pu_ctrl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_get_picture_quality_setting) for drv_param_get_picture_quality_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_gain) for drv_vidc_set_gain
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_enh_lum) for drv_vidc_set_enh_lum
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_enh_chr) for drv_vidc_set_enh_chr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_enh_chr2) for drv_vidc_set_enh_chr2
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter) for drv_dsc_dec_convert_pps_rc_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header) for drv_rxbr_set_ack_pkt_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) for hal_internal_vsync_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_pq_enh_chr) refers to drv_vidc.o(i.drv_vidc_set_enh_chr) for drv_vidc_set_enh_chr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_pq_enh_chr) refers to drv_param_init.o(i.drv_param_set_enh_chr) for drv_param_set_enh_chr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_pq_enh_chr) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_pq_enh_chr2) refers to drv_vidc.o(i.drv_vidc_set_enh_chr2) for drv_vidc_set_enh_chr2
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_pq_enh_chr2) refers to drv_param_init.o(i.drv_param_set_enh_chr2) for drv_param_set_enh_chr2
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_pq_enh_chr2) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_pq_enh_lum) refers to drv_vidc.o(i.drv_vidc_set_enh_lum) for drv_vidc_set_enh_lum
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_pq_enh_lum) refers to drv_param_init.o(i.drv_param_set_enh_lum) for drv_param_set_enh_lum
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_pq_enh_lum) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_pq_gain) refers to drv_vidc.o(i.drv_vidc_set_gain) for drv_vidc_set_gain
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_pq_gain) refers to drv_param_init.o(i.drv_param_set_gain) for drv_param_set_gain
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_pq_gain) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef0) for drv_vidc_set_scld_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef1) for drv_vidc_set_scld_hcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef0) for drv_vidc_set_scld_vcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef1) for drv_vidc_set_scld_vcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_param_init.o(i.drv_param_init_set_scld_filter) for drv_param_init_set_scld_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) for hal_internal_vsync_set_sync_line
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg) for drv_rxbr_hline_rcv0_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_dcs_direct_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode) for hal_internal_vsync_set_dcs_direct_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) refers to drv_rxbr.o(i.drv_rxbr_set_cmd_filter) for drv_rxbr_set_cmd_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) for drv_dsi_rx_calc_ipi_tx_delay
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg) for drv_dsi_rx_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format) refers to drv_vidc.o(i.drv_vidc_update_src_format) for drv_vidc_update_src_format
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format) refers to drv_vidc.o(i.drv_vidc_set_pentile_swap) for drv_vidc_set_pentile_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) for hal_dsi_rx_ctrl_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_src) for drv_crgu_set_rxbr_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_div) for drv_crgu_set_rxbr_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_dsco_src) for drv_crgu_set_dsco_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_dsco_src_div) for drv_crgu_set_dsco_src_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_dsc_core_div) for drv_crgu_set_dsc_core_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_te_waveform) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_te_waveform) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_dsi_rx.o(i.drv_dsi_rx_power_up) for drv_dsi_rx_power_up
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) for hal_internal_vsync_get_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg) for drv_rxbr_hline_rcv0_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) for hal_internal_sync_input_resolution_change
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fscalb.o(.text) for __ARM_scalbnf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fflti.o(.text) for __aeabi_i2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to ffixi.o(.text) for __aeabi_f2iz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk) for drv_dsi_tx_set_video_chunk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing) for drv_dsi_tx_set_video_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to drv_phy_common.o(i.drv_phy_get_rate_para) for drv_phy_get_rate_para
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to fadd.o(.text) for __aeabi_fsub
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to ffixui.o(.text) for __aeabi_f2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) for hal_lcdc_config_upscaler
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to drv_lcdc.o(i.drv_lcdc_config_src_parameter) for drv_lcdc_config_src_parameter
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_ulps_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) for drv_dsi_tx_phy_ulps_enter
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_ulps_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) for drv_dsi_tx_phy_ulps_exit
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) for hal_dsi_tx_ctrl_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_tx) for hal_internal_vsync_init_tx
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate) for hal_dsi_tx_config_params_for_lane_rate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) for hal_dsi_tx_count_lane_rate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) for hal_dsi_tx_init_phy_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) for drv_dsi_tx_phy_test_setup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) for hal_lcdc_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) for hal_lcdc_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) for hal_dsi_tx_init_dpi_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) for hal_dsi_tx_init_data_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) for hal_dsi_tx_init_remains
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt) for hal_dsi_tx_init_interrupt
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready) for drv_dsi_tx_phy_status_ready
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload) for drv_dsi_tx_command_get_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) refers to drv_param_init.o(i.drv_param_init_set_ccm) for drv_param_init_set_ccm
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_pq_edge) refers to drv_lcdc.o(i.drv_lcdc_config_yuv420_threshold) for drv_lcdc_config_yuv420_threshold
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_pq_filter) refers to drv_lcdc.o(i.drv_lcdc_config_sclu_filter) for drv_lcdc_config_sclu_filter
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness) refers to drv_lcdc.o(i.drv_lcdc_config_endianness) for drv_lcdc_config_endianness
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_horizon_flip) refers to drv_lcdc.o(i.drv_lcdc_config_horiz_flip) for drv_lcdc_config_horiz_flip
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_lp_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd) for drv_dsi_tx_video_mode_set_lp_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb) for drv_lcdc_config_overwrite_rgb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp) refers to drv_lcdc.o(i.drv_lcdc_config_partial_display_enable) for drv_lcdc_config_partial_display_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area) refers to drv_lcdc.o(i.drv_lcdc_config_partial_display_area) for drv_lcdc_config_partial_display_area
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_vpg) for drv_dsi_tx_set_vpg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_enable_shadow_reg) for drv_lcdc_enable_shadow_reg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_start) for drv_lcdc_start
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_lcdc.o(i.drv_lcdc_start) for drv_lcdc_start
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) for hal_dsi_tx_init_video_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode) for drv_dsi_tx_dpi_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity) for drv_dsi_tx_dpi_polarity
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time) for drv_dsi_tx_dpi_lpcmd_time
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_int) for drv_dsi_tx_config_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode) for drv_dsi_tx_phy_lane_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg) for drv_dsi_tx_phy_time_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_response_mode) for drv_dsi_tx_response_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div) for drv_dsi_tx_set_time_out_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg) for drv_dsi_tx_timeout_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp) for drv_dsi_tx_phy_clock_lane_auto_lp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg) for drv_dsi_tx_video_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack) for drv_dsi_tx_set_bta_ack
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd) for drv_dsi_tx_video_mode_set_lp_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_disable_hact_cmd) for drv_dsi_tx_video_mode_disable_hact_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) for hal_dsi_tx_calc_video_chunks
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_header) for drv_dsi_tx_command_header
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) refers to drv_param_init.o(i.drv_param_init_get_ccm) for drv_param_init_get_ccm
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) refers to drv_lcdc.o(i.drv_lcdc_config_ccm) for drv_lcdc_config_ccm
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_disp_mode) for drv_lcdc_config_disp_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_endianness) for drv_lcdc_config_endianness
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_horiz_flip) for drv_lcdc_config_horiz_flip
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_cbcr) for drv_lcdc_config_cbcr
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_thresh) for drv_lcdc_config_thresh
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_dpi_polarity) for drv_lcdc_config_dpi_polarity
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_src_parameter) for drv_lcdc_config_src_parameter
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_y2t4_use_sclu) for hal_internal_vsync_get_y2t4_use_sclu
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_lcdc.o(i.drv_lcdc_config_yuv420_threshold) for drv_lcdc_config_yuv420_threshold
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_lcdc.o(i.drv_lcdc_config_420_to_444_mode) for drv_lcdc_config_420_to_444_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area) for hal_dsi_tx_ctrl_set_partial_disp_area
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp) for hal_dsi_tx_ctrl_set_partial_disp
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_lcdc.o(i.drv_lcdc_config_upscaler) for drv_lcdc_config_upscaler
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_yuv_to_rgb) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) for hal_lcdc_config_upscaler
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_yuv_to_rgb) for hal_lcdc_config_yuv_to_rgb
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) for hal_lcdc_config_ccm
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile) for hal_lcdc_config_rgb_to_pentile
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) for hal_lcdc_config_remains
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) for hal_lcdc_init_interrupt
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dpi_pre_div) for drv_crgu_set_dpi_pre_div
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dpi_pre_src) for drv_crgu_set_dpi_pre_src
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dpi_mux_src) for drv_crgu_set_dpi_mux_src
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_lcdc.o(i.drv_lcdc_config_dpi_timing) for drv_lcdc_config_dpi_timing
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to cfrcmple.o(.text) for __aeabi_cfrcmple
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ffixi.o(.text) for __aeabi_f2iz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_lcdc_div) for drv_crgu_set_lcdc_div
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_lcdc_src) for drv_crgu_set_lcdc_src
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to drv_lcdc.o(i.drv_lcdc_ctrl_flow) for drv_lcdc_ctrl_flow
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to drv_lcdc.o(i.drv_lcdc_config_int) for drv_lcdc_config_int
    hal_gpio.o(i.hal_gpio_ctrl_eint) refers to drv_gpio.o(i.drv_gpio_set_int) for drv_gpio_set_int
    hal_gpio.o(i.hal_gpio_ctrl_eint) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_get_input_data) refers to drv_gpio.o(i.drv_gpio_get_input_data) for drv_gpio_get_input_data
    hal_gpio.o(i.hal_gpio_get_int_type) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to drv_gpio.o(i.drv_gpio_get_pull_state) for drv_gpio_get_pull_state
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_eint) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group) for drv_sys_cfg_sel_gpio_group
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig) for drv_sys_cfg_sel_int_trig
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_init_eint) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_input) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_input) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_input) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_init_output) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_reg_eint_cb) refers to drv_gpio.o(i.drv_gpio_register_callback) for drv_gpio_register_callback
    hal_gpio.o(i.hal_gpio_reg_eint_cb) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_gpio.o(i.drv_gpio_register_ap_reset_callback) for drv_gpio_register_ap_reset_callback
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) for drv_sys_cfg_sel_ap_rst_trig
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to drv_gpio.o(i.drv_gpio_set_driving_strength) for drv_gpio_set_driving_strength
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode3) for drv_gpio_set_mode3
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode2) for drv_gpio_set_mode2
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode1) for drv_gpio_set_mode1
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode0) for drv_gpio_set_mode0
    hal_gpio.o(i.hal_gpio_set_mode) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_output_data) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to drv_gpio.o(i.drv_gpio_set_pull_state) for drv_gpio_set_pull_state
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to drv_gpio.o(i.drv_gpio_set_schmitt_trigger) for drv_gpio_set_schmitt_trigger
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to drv_gpio.o(i.drv_gpio_set_slew_rate) for drv_gpio_set_slew_rate
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to hal_gpio.o(.constdata) for .constdata
    hal_i2c_master.o(i.hal_i2c_m_deinit) refers to drv_i2c_master.o(i.drv_i2c_m_deinit) for drv_i2c_m_deinit
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_master.o(i.drv_i2c_master_init) for drv_i2c_master_init
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_master.o(i.drv_i2c_m_set_callback) for drv_i2c_m_set_callback
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_master.o(i.drv_i2c_m_enable_intr) for drv_i2c_m_enable_intr
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_dma.o(i.drv_i2c_dma_init) for drv_i2c_dma_init
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_dma.o(i.drv_i2c_enable_rx_dma) for drv_i2c_enable_rx_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_dma.o(i.drv_i2c_enable_tx_dma) for drv_i2c_enable_tx_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to hal_i2c_master.o(i.hal_i2c_master_irq_callback) for hal_i2c_master_irq_callback
    hal_i2c_master.o(i.hal_i2c_m_dma_read) refers to drv_i2c_dma.o(i.drv_i2c_master_read_dma) for drv_i2c_master_read_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_read) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_master.o(i.hal_i2c_m_dma_write) refers to drv_i2c_dma.o(i.drv_i2c_master_write_dma) for drv_i2c_master_write_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_write) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_master.o(i.hal_i2c_m_set_high_impedance) refers to drv_i2c_master.o(i.drv_i2c_m_enable) for drv_i2c_m_enable
    hal_i2c_master.o(i.hal_i2c_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_master.o(i.hal_i2c_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_i2c_master.o(i.hal_i2c_m_transfer_complate) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_master.o(i.hal_i2c_master_irq_callback) refers to drv_i2c_master.o(i.drv_i2c_clear_m_it_pending_bit) for drv_i2c_clear_m_it_pending_bit
    hal_i2c_master.o(i.hal_i2c_master_irq_callback) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to drv_i2c_slave.o(i.drv_i2c_s_deinit) for drv_i2c_s_deinit
    hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to drv_i2c_dma.o(i.drv_i2c_slave_write_dma) for drv_i2c_slave_write_dma
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_get_tx_byte_num) refers to drv_i2c_slave.o(i.drv_i2c_s_get_tx_byte_num) for drv_i2c_s_get_tx_byte_num
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c_slave_init) for drv_i2c_slave_init
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c_s_set_callback) for drv_i2c_s_set_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c_s_enable_intr) for drv_i2c_s_enable_intr
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_dma.o(i.drv_i2c_dma_init) for drv_i2c_dma_init
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) for drv_i2c_set_dma_irq_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_dma.o(i.drv_i2c_enable_tx_dma) for drv_i2c_enable_tx_dma
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_dma.o(i.drv_dma_enable_cycle) for drv_dma_enable_cycle
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) for hal_i2c_slave_irq_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback) for hal_i2c_s_dma_user_callback
    hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_complate) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_complate_clear) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_data) refers to drv_i2c_slave.o(i.drv_i2c_s_read_data) for drv_i2c_s_read_data
    hal_i2c_slave.o(i.hal_i2c_s_rxfifo_notempty) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    hal_i2c_slave.o(i.hal_i2c_s_set_dma_tx_cycle) refers to drv_dma.o(i.drv_dma_enable_cycle) for drv_dma_enable_cycle
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to drv_i2c_slave.o(i.drv_i2c_s_enable) for drv_i2c_s_enable
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_i2c_slave.o(i.hal_i2c_s_set_transfer) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_write_complate) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_write_data) refers to drv_i2c_slave.o(i.drv_i2c_s_write_data) for drv_i2c_s_write_data
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(i.drv_i2c_clear_s_it_pending_bit) for drv_i2c_clear_s_it_pending_bit
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(i.drv_i2c_s_write_data) for drv_i2c_s_write_data
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(.data) for tx_byte_num
    hal_spi_master.o(i.hal_spi_m_callback) refers to drv_spi_dma.o(i.drv_spi_abort_dma) for drv_spi_abort_dma
    hal_spi_master.o(i.hal_spi_m_callback) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_clear_rxfifo) refers to drv_spi_master.o(i.drv_spi_m_read_data) for drv_spi_m_read_data
    hal_spi_master.o(i.hal_spi_m_deinit) refers to drv_spi_master.o(i.drv_spi_m_deinit) for drv_spi_m_deinit
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to hal_spi_master.o(i.hal_spi_m_gpio_init) for hal_spi_m_gpio_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_master.o(i.drv_spi_master_init) for drv_spi_master_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_dma_init) for drv_spi_dma_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) for drv_spi_set_dma_irq_callback
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_master.o(i.drv_spi_m_enable_rx_dma) for drv_spi_m_enable_rx_dma
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to hal_spi_master.o(i.hal_spi_m_callback) for hal_spi_m_callback
    hal_spi_master.o(i.hal_spi_m_dma_read) refers to drv_spi_dma.o(i.drv_spim_dma_read) for drv_spim_dma_read
    hal_spi_master.o(i.hal_spi_m_dma_read) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_dma_write) refers to drv_spi_dma.o(i.drv_spim_dma_write) for drv_spim_dma_write
    hal_spi_master.o(i.hal_spi_m_dma_write) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_get_transfer_complate) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_gpio_init) refers to drv_spi_master.o(i.drv_spi_m_gpio_init) for drv_spi_m_gpio_init
    hal_spi_master.o(i.hal_spi_m_set_high_impedance) refers to drv_spi_master.o(i.drv_spi_m_enable) for drv_spi_m_enable
    hal_spi_master.o(i.hal_spi_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_spi_master.o(i.hal_spi_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    hal_spi_master.o(i.hal_spi_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_swire.o(i.hal_swire_deinit) refers to drv_swire.o(i.drv_swire_enable) for drv_swire_enable
    hal_swire.o(i.hal_swire_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_swire.o(i.hal_swire_init) refers to drv_crgu.o(i.drv_crgu_set_swire_div) for drv_crgu_set_swire_div
    hal_swire.o(i.hal_swire_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_swire.o(i.hal_swire_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_swire.o(i.hal_swire_init) refers to drv_swire.o(i.drv_swire_enable) for drv_swire_enable
    hal_swire.o(i.hal_swire_open) refers to drv_swire.o(i.drv_swire_set_power_down) for drv_swire_set_power_down
    hal_swire.o(i.hal_swire_register_callback) refers to drv_swire.o(i.drv_swire_register_callback) for drv_swire_register_callback
    hal_swire.o(i.hal_swire_start) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    hal_swire.o(i.hal_swire_start) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_swire.o(i.hal_swire_start) refers to drv_swire.o(i.drv_swire_set_bit_time) for drv_swire_set_bit_time
    hal_swire.o(i.hal_swire_start) refers to drv_swire.o(i.drv_swire_set_pulse_count) for drv_swire_set_pulse_count
    hal_swire.o(i.hal_swire_start) refers to drv_common.o(.data) for g_system_clock
    hal_system.o(i.hal_system_deep_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode) for drv_pwr_enter_deep_sleep_mode
    hal_system.o(i.hal_system_disable_systick) refers to drv_common.o(i.drv_common_disable_systick) for drv_common_disable_systick
    hal_system.o(i.hal_system_enable_systick) refers to drv_common.o(i.drv_common_enable_systick) for drv_common_enable_systick
    hal_system.o(i.hal_system_flash_read) refers to norflash.o(i.norflash_init) for norflash_init
    hal_system.o(i.hal_system_flash_read) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    hal_system.o(i.hal_system_flash_read) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_system.o(i.hal_system_flash_read) refers to norflash.o(i.norflash_dual_read) for norflash_dual_read
    hal_system.o(i.hal_system_flash_write) refers to norflash.o(i.norflash_init) for norflash_init
    hal_system.o(i.hal_system_flash_write) refers to norflash.o(i.norflash_erase_block) for norflash_erase_block
    hal_system.o(i.hal_system_flash_write) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_system.o(i.hal_system_flash_write) refers to norflash.o(i.norflash_write) for norflash_write
    hal_system.o(i.hal_system_get_tick) refers to drv_common.o(i.drv_common_get_tick) for drv_common_get_tick
    hal_system.o(i.hal_system_idle_mode) refers to drv_common.o(i.drv_common_idle_mode) for drv_common_idle_mode
    hal_system.o(i.hal_system_init) refers to drv_pwr.o(i.drv_pwr_set_system_clk_src) for drv_pwr_set_system_clk_src
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_set_ahb_src) for drv_crgu_set_ahb_src
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_set_ahb_pre_div) for drv_crgu_set_ahb_pre_div
    hal_system.o(i.hal_system_init) refers to irq_redirect .o(i.handle_init) for handle_init
    hal_system.o(i.hal_system_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int) for drv_sys_cfg_clear_all_int
    hal_system.o(i.hal_system_init) refers to drv_common.o(i.drv_common_system_init) for drv_common_system_init
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_system.o(i.hal_system_init) refers to drv_pwr.o(i.drv_pwr_set_pvd_mode) for drv_pwr_set_pvd_mode
    hal_system.o(i.hal_system_init) refers to drv_common.o(.data) for g_system_clock
    hal_system.o(i.hal_system_init_console) refers to hal_uart.o(i.hal_uart_init) for hal_uart_init
    hal_system.o(i.hal_system_register_systick_cb) refers to drv_common.o(i.drv_common_systick_register_cb) for drv_common_systick_register_cb
    hal_system.o(i.hal_system_set_pvd) refers to drv_pwr.o(i.drv_pwr_set_pvd_mode) for drv_pwr_set_pvd_mode
    hal_system.o(i.hal_system_set_vcc) refers to drv_pwr.o(i.drv_pwr_set_cp_mode) for drv_pwr_set_cp_mode
    hal_system.o(i.hal_system_share_flash_mode) refers to drv_fls.o(i.drv_fls_gpio_connect) for drv_fls_gpio_connect
    hal_system.o(i.hal_system_share_flash_mode) refers to drv_fls.o(i.drv_fls_gpio_disconnect) for drv_fls_gpio_disconnect
    hal_system.o(i.hal_system_sleep_mode) refers to drv_crgu.o(i.drv_crgu_config_clocks) for drv_crgu_config_clocks
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_set_repeat) for drv_timer_set_repeat
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_timer.o(i.hal_timer_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_timer.o(i.hal_timer_get_status) refers to drv_timer.o(i.drv_timer_get_status) for drv_timer_get_status
    hal_timer.o(i.hal_timer_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_timer.o(i.hal_timer_init) refers to drv_timer.o(i.drv_timer_set_prescaler) for drv_timer_set_prescaler
    hal_timer.o(i.hal_timer_set_repeat) refers to drv_timer.o(i.drv_timer_set_repeat) for drv_timer_set_repeat
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_get_prescaler) for drv_timer_get_prescaler
    hal_timer.o(i.hal_timer_start) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_start) refers to drv_common.o(.data) for g_system_clock
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_get_prescaler) for drv_timer_get_prescaler
    hal_timer.o(i.hal_timer_start_ex) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_start_ex) refers to drv_common.o(.data) for g_system_clock
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    tau_delay.o(i.delayMs) refers to tau_delay.o(i.delayUs) for delayUs
    tau_log.o(i.LOG_printf) refers to printfa.o(i.__0vsprintf) for vsprintf
    tau_log.o(i.LOG_printf) refers to printfa.o(i.__0printf) for __2printf
    tau_log.o(i.LOG_printf) refers to tau_log.o(.bss) for .bss
    tau_log.o(i.fgetc) refers to hal_uart.o(i.hal_uart_receive_blocking) for hal_uart_receive_blocking
    tau_log.o(i.fputc) refers to hal_uart.o(i.hal_uart_transmit_blocking) for hal_uart_transmit_blocking
    norflash.o(i.app_fls_ctrl_Handler) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    norflash.o(i.app_fls_ctrl_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    norflash.o(i.app_fls_ctrl_Handler) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_best_cfg_init) refers to drv_fls.o(i.fls_spi_init) for fls_spi_init
    norflash.o(i.norflash_best_cfg_init) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_check_id) refers to norflash.o(i.norflash_read_id) for norflash_read_id
    norflash.o(i.norflash_check_id) refers to tau_delay.o(i.delayUs) for delayUs
    norflash.o(i.norflash_check_id) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dma_callback) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dma_read) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_transfer_create_handle_dma) for fls_transfer_create_handle_dma
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_dma_read_prepare) for fls_dma_read_prepare
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_transfer_dma) for fls_transfer_dma
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    norflash.o(i.norflash_dma_read) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dma_read) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_dma_read) refers to norflash.o(i.norflash_dma_callback) for norflash_dma_callback
    norflash.o(i.norflash_dma_write) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_transfer_create_handle_dma) for fls_transfer_create_handle_dma
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_switch_fls_spi) for norflash_switch_fls_spi
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_dma_write_prepare) for fls_dma_write_prepare
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_transfer_dma) for fls_transfer_dma
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    norflash.o(i.norflash_dma_write) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_dma_write) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_dma_callback) for norflash_dma_callback
    norflash.o(i.norflash_dma_write) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dual_read) refers to drv_fls.o(i.fls_ddat_enable) for fls_ddat_enable
    norflash.o(i.norflash_dual_read) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_dual_read) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_switch_fls_spi) for norflash_switch_fls_spi
    norflash.o(i.norflash_dual_write) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_dual_write) refers to drv_fls.o(i.fls_ddat_enable) for fls_ddat_enable
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_en4b) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_read_config_reg) for norflash_read_config_reg
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_en_quad) refers to norflash.o(i.norflash_en_quad_check) for norflash_en_quad_check
    norflash.o(i.norflash_en_quad) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_en_quad) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_en_quad) refers to drv_fls.o(i.fls_busy_pending) for fls_busy_pending
    norflash.o(i.norflash_en_quad) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(i.norflash_get_dual_hstatus) for norflash_get_dual_hstatus
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(i.norflash_get_hstatus) for norflash_get_hstatus
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_erase_block) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_erase_block) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_erase_block) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_erase_block) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_erase_chip) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_erase_chip) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_erase_chip) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_erase_sector) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_erase_sector) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_erase_sector) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_erase_sector) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_ex4b) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_read_config_reg) for norflash_read_config_reg
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_exit_quad) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_exit_quad) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_exit_quad) refers to norflash.o(i.norflash_en_quad_check) for norflash_en_quad_check
    norflash.o(i.norflash_exit_quad) refers to drv_fls.o(i.fls_busy_pending) for fls_busy_pending
    norflash.o(i.norflash_exit_quad) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_get_dual_hstatus) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_get_dual_hstatus) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_get_dual_hstatus) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_get_hstatus) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_get_hstatus) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_get_hstatus) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_get_status) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_get_status) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_get_status) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_get_default_spi_config) for fls_get_default_spi_config
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_get_default_fls_config) for fls_get_default_fls_config
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_get_default_tuning) for fls_get_default_tuning
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_init) for fls_init
    norflash.o(i.norflash_init) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_init) refers to drv_fls.o(.data) for g_fls_tuning
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_qdat_enable) for fls_qdat_enable
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_qadr_enable) for fls_qadr_enable
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_qcmd_enable) for fls_qcmd_enable
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_switch_fls_spi) for norflash_switch_fls_spi
    norflash.o(i.norflash_quad_write) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_quad_write) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_read) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_read_config_reg) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_read_id) refers to drv_fls.o(i.fls_read_cmd) for fls_read_cmd
    norflash.o(i.norflash_set_best_cfg) refers to memseta.o(.text) for __aeabi_memclr4
    norflash.o(i.norflash_set_best_read_cfg) refers to norflash.o(i.norflash_en_quad) for norflash_en_quad
    norflash.o(i.norflash_set_best_read_cfg) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_set_best_read_cfg) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_set_best_write_cfg) refers to norflash.o(i.norflash_en_quad) for norflash_en_quad
    norflash.o(i.norflash_set_best_write_cfg) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_set_best_write_cfg) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_ddat_enable) for fls_ddat_enable
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_qdat_enable) for fls_qdat_enable
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_qadr_enable) for fls_qadr_enable
    norflash.o(i.norflash_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_write) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_write_disable) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_write_disable) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write_disable) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_write_disable) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_write_enable) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_write_enable) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write_enable) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_write_enable) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_big_end_enable) for norflash_big_end_enable
    norflash.o(i.norflash_write_endian_scr) refers to drv_fls.o(i.fls_en_scr) for fls_en_scr
    norflash.o(i.norflash_write_endian_scr) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_big_end_clear) for norflash_big_end_clear
    norflash.o(i.norflash_write_endian_scr) refers to drv_fls.o(i.fls_scr_clear) for fls_scr_clear
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    hal_uart.o(i.hal_uart_deinit) refers to drv_dma.o(i.drv_dma_deinit) for drv_dma_deinit
    hal_uart.o(i.hal_uart_deinit) refers to drv_uart.o(i.UART_Deinit) for UART_Deinit
    hal_uart.o(i.hal_uart_dmacallback) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_uart.o(i.hal_uart_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_uart.o(i.hal_uart_init) refers to drv_uart.o(i.UART_init) for UART_init
    hal_uart.o(i.hal_uart_init) refers to drv_common.o(.data) for g_system_clock
    hal_uart.o(i.hal_uart_init) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_receive_blocking) refers to drv_uart.o(i.UART_ReadBlocking) for UART_ReadBlocking
    hal_uart.o(i.hal_uart_receive_dma) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    hal_uart.o(i.hal_uart_receive_dma) refers to drv_uart_dma.o(i.UART_TransferCreateHandleDMA) for UART_TransferCreateHandleDMA
    hal_uart.o(i.hal_uart_receive_dma) refers to drv_uart_dma.o(i.UART_TransferReceiveDMA) for UART_TransferReceiveDMA
    hal_uart.o(i.hal_uart_receive_dma) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_receive_dma) refers to hal_uart.o(i.hal_uart_dmacallback) for hal_uart_dmacallback
    hal_uart.o(i.hal_uart_transmit_blocking) refers to drv_uart.o(i.UART_WriteBlocking) for UART_WriteBlocking
    hal_uart.o(i.hal_uart_transmit_dma) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    hal_uart.o(i.hal_uart_transmit_dma) refers to drv_uart_dma.o(i.UART_TransferCreateHandleDMA) for UART_TransferCreateHandleDMA
    hal_uart.o(i.hal_uart_transmit_dma) refers to drv_uart_dma.o(i.UART_TransferSendDMA) for UART_TransferSendDMA
    hal_uart.o(i.hal_uart_transmit_dma) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_transmit_dma) refers to hal_uart.o(i.hal_uart_dmacallback) for hal_uart_dmacallback
    drv_common.o(i.app_HardFault_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_common.o(i.app_SysTick_Handler) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_enable_systick) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_common.o(i.drv_common_enable_systick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_get_tick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_system_init) refers to drv_chip_info.o(i.drv_chip_info_init) for drv_chip_info_init
    drv_common.o(i.drv_common_system_init) refers to drv_chip_info.o(i.drv_chip_info_get_version) for drv_chip_info_get_version
    drv_common.o(i.drv_common_systick_register_cb) refers to drv_common.o(.data) for .data
    drv_dma.o(i.app_dma_irq_handler) refers to drv_dma.o(i.drv_dma_irq_handler) for drv_dma_irq_handler
    drv_dma.o(i.drv_dma_abort_transfer) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_abort_transfer) refers to drv_dma.o(i.drv_dma_disenable_channel_interrupts) for drv_dma_disenable_channel_interrupts
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_disenable_channel_interrupts) for drv_dma_disenable_channel_interrupts
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_clear_flag) for drv_dma_clear_flag
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_set_ccr) for drv_dma_set_ccr
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_dma.o(i.drv_dma_clear_flag) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.drv_dma_create_handle) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dma.o(i.drv_dma_disenable_channel_interrupts) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.drv_dma_enable_channel_interrupts) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dma.o(i.drv_dma_enable_cycle) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_get_remaining_bytes) refers to drv_dma.o(i.drv_dma_channel_is_active) for drv_dma_channel_is_active
    drv_dma.o(i.drv_dma_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dma.o(i.drv_dma_init) refers to drv_dma.o(i.drv_dma_ahb_init) for drv_dma_ahb_init
    drv_dma.o(i.drv_dma_irq_handler) refers to drv_dma.o(i.drv_dma_get_channel_flag) for drv_dma_get_channel_flag
    drv_dma.o(i.drv_dma_irq_handler) refers to drv_dma.o(i.drv_dma_clear_flag) for drv_dma_clear_flag
    drv_dma.o(i.drv_dma_irq_handler) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_m2m_init) refers to memseta.o(.text) for __aeabi_memclr4
    drv_dma.o(i.drv_dma_m2m_init) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    drv_dma.o(i.drv_dma_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_dma.o(i.drv_dma_set_burst) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_set_transfer) refers to drv_dma.o(i.drv_dma_set_burst) for drv_dma_set_burst
    drv_dma.o(i.drv_dma_start_transfer) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    drv_dma.o(i.drv_dma_start_transfer) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_fls.o(i.drv_fls_gpio_connect) refers to drv_fls.o(i.drv_fls_gpio_disconnect) for drv_fls_gpio_disconnect
    drv_fls.o(i.drv_fls_gpio_disconnect) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_EnableClk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_busy_pending) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    drv_fls.o(i.fls_de_init) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    drv_fls.o(i.fls_de_init) refers to drv_dma.o(i.drv_dma_clear_flag) for drv_dma_clear_flag
    drv_fls.o(i.fls_de_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_disable_it) refers to drv_fls.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_fls.o(i.fls_disable_it) refers to drv_fls.o(i.fls_set_irq_mask) for fls_set_irq_mask
    drv_fls.o(i.fls_enable_it) refers to drv_fls.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_fls.o(i.fls_enable_it) refers to drv_fls.o(i.fls_set_irq_mask) for fls_set_irq_mask
    drv_fls.o(i.fls_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_init) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_spi_init) for fls_spi_init
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_ctrl_cfg_init) for fls_ctrl_cfg_init
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_set_tuning) for fls_set_tuning
    drv_fls.o(i.fls_init) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_enable_it) for fls_enable_it
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_set_irq_mask) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_fls.o(i.fls_set_irq_mask) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_set_write) for fls_set_write
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_set_write) for fls_set_write
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect) for drv_ap_rst_trig_edge_detect
    drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_get_pull_state) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_register_ap_reset_callback) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.drv_gpio_register_callback) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_set_driving_strength) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_gpio.o(i.drv_gpio_set_pull_state) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_set_schmitt_trigger) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_set_slew_rate) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_i2c_dma.o(i.drv_i2c_dma_callback) refers to drv_i2c_dma.o(.data) for .data
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req) for drv_sys_cfg_set_dma_rx_req
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_dma.o(i.drv_dma_set_transfer) for drv_dma_set_transfer
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_i2c_dma.o(i.drv_i2c_master_write_read_cmd) for drv_i2c_master_write_read_cmd
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_dma.o(i.drv_dma_set_transfer) for drv_dma_set_transfer
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_i2c_dma.o(.data) for .data
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_i2c_dma.o(.bss) for .bss
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_i2c_dma.o(i.drv_i2c_dma_callback) for drv_i2c_dma_callback
    drv_i2c_dma.o(i.drv_i2c_slave_write_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_i2c_master.o(i.app_I2C1_IRQn_Handler) refers to drv_i2c_master.o(.data) for .data
    drv_i2c_master.o(i.drv_i2c_clear_m_it_pending_bit) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_i2c_master.o(i.drv_i2c_clear_m_it_pending_bit) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_enable_intr) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_read_data) refers to drv_i2c_master.o(i.drv_i2c_m_get_fifo_status) for drv_i2c_m_get_fifo_status
    drv_i2c_master.o(i.drv_i2c_m_set_callback) refers to drv_i2c_master.o(.data) for .data
    drv_i2c_master.o(i.drv_i2c_m_set_sys_mask) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_write_data) refers to drv_i2c_master.o(i.drv_i2c_m_get_fifo_status) for drv_i2c_m_get_fifo_status
    drv_i2c_master.o(i.drv_i2c_master_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_i2c_master.o(i.drv_i2c_master_init) refers to drv_common.o(.data) for g_system_clock
    drv_i2c_slave.o(i.app_I2C0_IRQn_Handler) refers to drv_i2c_slave.o(.data) for .data
    drv_i2c_slave.o(i.drv_i2c_clear_s_it_pending_bit) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_i2c_slave.o(i.drv_i2c_clear_s_it_pending_bit) refers to drv_i2c_slave.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_slave.o(i.drv_i2c_s_enable_intr) refers to drv_i2c_slave.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_slave.o(i.drv_i2c_s_get_tx_byte_num) refers to drv_i2c_slave.o(.data) for .data
    drv_i2c_slave.o(i.drv_i2c_s_read_data) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    drv_i2c_slave.o(i.drv_i2c_s_set_callback) refers to drv_i2c_slave.o(.data) for .data
    drv_i2c_slave.o(i.drv_i2c_s_set_sys_mask) refers to drv_i2c_slave.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_slave.o(i.drv_i2c_s_write_data) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    drv_param_init.o(i.drv_param_get_picture_quality_setting) refers to memcpya.o(.text) for __aeabi_memcpy4
    drv_param_init.o(i.drv_param_get_picture_quality_setting) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_get_ccm) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_get_scld_filter_h) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_get_scld_filter_v) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_get_sclu_filter_h) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_get_sclu_filter_v) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_set_ccm) refers to memcpya.o(.text) for __aeabi_memcpy4
    drv_param_init.o(i.drv_param_init_set_ccm) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_set_scld_filter) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_set_sclu_filter) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_p2r_filter_init) refers to memcpya.o(.text) for __aeabi_memcpy4
    drv_param_init.o(i.drv_param_p2r_filter_init) refers to drv_param_init.o(.constdata) for .constdata
    drv_param_init.o(i.drv_param_set_enh_chr) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_set_enh_chr2) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_set_enh_lum) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_set_gain) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_yuv420_filter_init) refers to drv_param_init.o(.constdata) for .constdata
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_dma.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_dma.o(i.drv_spi_dma_callback) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_dma_init) refers to drv_spi_dma.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_spi_dma.o(i.drv_spi_dma_callback) for drv_spi_dma_callback
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req) for drv_sys_cfg_set_dma_rx_req
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_dma.o(i.drv_dma_set_transfer) for drv_dma_set_transfer
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_dma.o(i.drv_dma_start_transfer) for drv_dma_start_transfer
    drv_spi_dma.o(i.drv_spim_dma_read) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_dma.o(i.drv_dma_set_transfer) for drv_dma_set_transfer
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_dma.o(i.drv_dma_start_transfer) for drv_dma_start_transfer
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_master.o(i.app_SPIM_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_spi_master.o(i.app_SPIM_IRQn_Handler) refers to drv_spi_master.o(.data) for .data
    drv_spi_master.o(i.drv_spi_m_disable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_spi_master.o(i.drv_spi_m_disable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_spi_master.o(i.drv_spi_m_enable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_spi_master.o(i.drv_spi_m_set_intr_callback) refers to drv_spi_master.o(.data) for .data
    drv_spi_master.o(i.drv_spi_master_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_spi_master.o(i.drv_spi_master_init) refers to drv_common.o(.data) for g_system_clock
    drv_swire.o(i.app_SWIRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_swire.o(i.app_SWIRE_IRQn_Handler) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    drv_swire.o(i.app_SWIRE_IRQn_Handler) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_register_callback) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig) for drv_sys_cfg_sel_ap_rst_lvl_trig
    drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect) refers to drv_sys_cfg.o(.data) for .data
    drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig) for drv_sys_cfg_sel_ap_rst_lvl_trig
    drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) refers to drv_sys_cfg.o(.data) for .data
    drv_timer.o(i.app_TIMER0_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.app_TIMER1_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.app_TIMER2_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.app_TIMER3_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_timer.o(i.drv_timer_enable) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_get_instance) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_get_prescaler) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_get_status) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_clear_status_flags) for drv_timer_clear_status_flags
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_register_callback) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_compare_val) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_repeat) refers to drv_timer.o(.data) for .data
    dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_fifo_init) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_size) refers to dcs_packet_fifo.o(.bss) for .bss
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to hal_internal_vsync.o(i.soft_gen_te) for soft_gen_te
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_param_init.o(i.drv_param_init_get_ccm) for drv_param_init_get_ccm
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_lcdc.o(i.drv_lcdc_config_ccm) for drv_lcdc_config_ccm
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_internal_vsync.o(i.app_VIDC_IRQn_Handler) refers to drv_vidc.o(i.drv_vidc_get_int_source) for drv_vidc_get_int_source
    hal_internal_vsync.o(i.app_VIDC_IRQn_Handler) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_internal_vsync.o(i.app_VIDC_IRQn_Handler) refers to drv_vidc.o(i.drv_vidc_clear_irq) for drv_vidc_clear_irq
    hal_internal_vsync.o(i.app_VIDC_IRQn_Handler) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_internal_vsync.o(i.app_VIDC_IRQn_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.app_VIDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_internal_vsync.o(i.app_VIDC_IRQn_Handler) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.app_VIDC_IRQn_Handler) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.app_VPRE_IRQn_Handler) refers to hal_internal_vsync.o(i.drv_rxbr_get_int_source) for drv_rxbr_get_int_source
    hal_internal_vsync.o(i.app_VPRE_IRQn_Handler) refers to hal_internal_vsync.o(i.rx_receive_packet) for rx_receive_packet
    hal_internal_vsync.o(i.app_VPRE_IRQn_Handler) refers to drv_rxbr.o(i.drv_rxbr_clear_status) for drv_rxbr_clear_status
    hal_internal_vsync.o(i.app_VPRE_IRQn_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.app_VPRE_IRQn_Handler) refers to hal_internal_vsync.o(i.vpre_err_reset) for vpre_err_reset
    hal_internal_vsync.o(i.app_VPRE_IRQn_Handler) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.app_VPRE_IRQn_Handler) refers to hal_internal_vsync.o(i.drv_rxbr_get_status) for drv_rxbr_get_status
    hal_internal_vsync.o(i.app_VPRE_IRQn_Handler) refers to drv_rxbr.o(i.drv_rxbr_get_cur_hline_rcv_cnt) for drv_rxbr_get_cur_hline_rcv_cnt
    hal_internal_vsync.o(i.app_VPRE_IRQn_Handler) refers to drv_rxbr.o(i.drv_rxbr_get_hline_rcv_cfg) for drv_rxbr_get_hline_rcv_cfg
    hal_internal_vsync.o(i.app_VPRE_IRQn_Handler) refers to drv_lcdc.o(i.drv_lcdc_update_shadow_reg) for drv_lcdc_update_shadow_reg
    hal_internal_vsync.o(i.app_VPRE_IRQn_Handler) refers to drv_lcdc.o(i.drv_lcdc_start) for drv_lcdc_start
    hal_internal_vsync.o(i.app_VPRE_IRQn_Handler) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_internal_vsync.o(i.app_VPRE_IRQn_Handler) refers to hal_internal_vsync.o(i.rx_partial_update) for rx_partial_update
    hal_internal_vsync.o(i.app_VPRE_IRQn_Handler) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.app_VPRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_internal_vsync.o(i.app_VPRE_IRQn_Handler) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.app_VPRE_IRQn_Handler) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) for hal_internal_sync_set_fb_setting_manual
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to hal_internal_vsync.o(i.drv_rxbr_get_status) for drv_rxbr_get_status
    hal_internal_vsync.o(i.dcs_sw_filter) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_hwclr) for drv_memc_set_tear_hwclr
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_yuv420_cfg) for drv_memc_set_yuv420_cfg
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_bypass_fifo_empty) for drv_memc_bypass_fifo_empty
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_rxbr.o(i.drv_rxbr_clear_status) for drv_rxbr_clear_status
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) for hal_dsi_rx_ctrl_gen_a_tear_signal
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_delay.o(i.delayUs) for delayUs
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.hal_internal_init_memc) for hal_internal_init_memc
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_y2t4_use_sclu) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_chip_info.o(i.drv_chip_rx_info_check) for drv_chip_rx_info_check
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_init) for dcs_packet_fifo_init
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) refers to drv_rxbr.o(i.drv_rxbr_set_cmd_filter) for drv_rxbr_set_cmd_filter
    hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) for hal_internal_vsync_set_auto_hw_filter
    hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(i.vsync_set_te_mode) for vsync_set_te_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.vsync_set_te_mode) for vsync_set_te_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(i.dcs_sw_filter) for dcs_sw_filter
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) for dcs_packet_fifo_alloc
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) for hal_dsi_rx_ctrl_dsc_async_handler
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_header) for drv_dsi_tx_command_header
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_rxbr.o(i.drv_rxbr_get_col_addr) for drv_rxbr_get_col_addr
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_rxbr.o(i.drv_rxbr_get_page_addr) for drv_rxbr_get_page_addr
    hal_internal_vsync.o(i.rx_partial_update) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_dsc_dec.o(i.drv_dsc_dec_get_nslc) for drv_dsc_dec_get_nslc
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_crgu.o(i.drv_crgu_set_dsco_src) for drv_crgu_set_dsco_src
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_crgu.o(i.drv_crgu_set_dsco_src_div) for drv_crgu_set_dsco_src_div
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_crgu.o(i.drv_crgu_set_dsc_core_div) for drv_crgu_set_dsc_core_div
    hal_internal_vsync.o(i.rx_partial_update) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(i.rx_get_dcs_packet_data) for rx_get_dcs_packet_data
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(i.rx_receive_pps) for rx_receive_pps
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(i.drv_rxbr_get_status) for drv_rxbr_get_status
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_receive_pps) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.rx_receive_pps) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rx_receive_pps) refers to hal_internal_vsync.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter) for drv_dsc_dec_convert_pps_rc_parameter
    hal_internal_vsync.o(i.rx_receive_pps) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps) for drv_dsc_dec_set_u8_pps
    hal_internal_vsync.o(i.rx_receive_pps) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.rx_receive_pps) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps) for drv_dsc_dec_set_u8_pps
    hal_internal_vsync.o(i.vpre_err_reset) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to drv_lcdc.o(i.drv_lcdc_ctrl_flow) for drv_lcdc_ctrl_flow
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(.data) refers to hal_internal_vsync.o(.bss) for sg_te_info
    drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to ffltui.o(.text) for __aeabi_ui2f
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fdiv.o(.text) for __aeabi_fdiv
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fmul.o(.text) for __aeabi_fmul
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) for drv_dsi_rx_get_color_bpp
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc) for drv_dsi_rx_get_color_pcc
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fadd.o(.text) for __aeabi_fadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to cfrcmple.o(.text) for __aeabi_cfrcmple
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to f2d.o(.text) for __aeabi_f2d
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dadd.o(.text) for __aeabi_dadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dfixui.o(.text) for __aeabi_d2uiz
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte) for drv_rx_phy_test_write_1_byte
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to drv_dsi_rx.o(i.drv_rx_phy_test_read) for drv_rx_phy_test_read
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_get_rate_para) for drv_phy_get_rate_para
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_clear) for drv_rx_phy_test_clear
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte) for drv_rx_phy_test_write_1_byte
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte) for drv_rx_phy_test_write_2_byte
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_lock) for drv_rx_phy_test_lock
    drv_dsi_rx.o(i.drv_rx_phy_test_clear) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_rx.o(i.drv_rx_phy_test_lock) refers to drv_phy_common.o(i.drv_phy_test_lock) for drv_phy_test_lock
    drv_dsi_rx.o(i.drv_rx_phy_test_read) refers to drv_phy_common.o(i.drv_phy_test_read) for drv_phy_test_read
    drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_1_byte) for drv_phy_test_write_1_byte
    drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_2_byte) for drv_phy_test_write_2_byte
    drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) for drv_tx_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to drv_dsi_tx.o(i.drv_tx_phy_test_read) for drv_tx_phy_test_read
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_get_rate_para) for drv_phy_get_rate_para
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_get_pll_para) for drv_phy_get_pll_para
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_enter) for drv_tx_phy_test_enter
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_crgu.o(i.drv_crgu_set_mipi_ref_src) for drv_crgu_set_mipi_ref_src
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_crgu.o(i.drv_crgu_set_mipi_cfg_src) for drv_crgu_set_mipi_cfg_src
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_clear) for drv_tx_phy_test_clear
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) for drv_tx_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte) for drv_tx_phy_test_write_2_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_code) for drv_tx_phy_test_write_code
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_exit) for drv_tx_phy_test_exit
    drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) for drv_tx_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_version) for drv_dsi_tx_version
    drv_dsi_tx.o(i.drv_dsi_tx_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dsi_tx.o(i.drv_tx_phy_test_clear) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_tx.o(i.drv_tx_phy_test_read) refers to drv_phy_common.o(i.drv_phy_test_read) for drv_phy_test_read
    drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_1_byte) for drv_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_2_byte) for drv_phy_test_write_2_byte
    drv_dsi_tx.o(i.drv_tx_phy_test_write_code) refers to drv_phy_common.o(i.drv_phy_test_write_code) for drv_phy_test_write_code
    drv_lcdc.o(i.drv_lcdc_config_src_parameter) refers to drv_lcdc.o(i.drv_lcdc_config_input_size) for drv_lcdc_config_input_size
    drv_lcdc.o(i.drv_lcdc_config_upscaler) refers to drv_param_init.o(i.drv_param_init_get_sclu_filter_h) for drv_param_init_get_sclu_filter_h
    drv_lcdc.o(i.drv_lcdc_config_upscaler) refers to drv_param_init.o(i.drv_param_init_get_sclu_filter_v) for drv_param_init_get_sclu_filter_v
    drv_lcdc.o(i.drv_lcdc_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_memc.o(i.app_MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_get_status) for drv_memc_get_status
    drv_memc.o(i.app_MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_clear_status) for drv_memc_clear_status
    drv_memc.o(i.app_MEMC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_phy_common.o(i.drv_phy_get_pll_para) refers to drv_phy_common.o(.constdata) for .constdata
    drv_phy_common.o(i.drv_phy_get_rate_para) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_phy_common.o(i.drv_phy_get_rate_para) refers to drv_phy_common.o(.constdata) for .constdata
    drv_phy_common.o(i.drv_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_code) for drv_phy_test_write_code
    drv_phy_common.o(i.drv_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_data) for drv_phy_test_write_data
    drv_phy_common.o(i.drv_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_code) for drv_phy_test_write_code
    drv_phy_common.o(i.drv_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_data) for drv_phy_test_write_data
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_rxbr.o(i.drv_rxbr_err_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_rxbr.o(i.drv_rxbr_set_cmd_filter) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_vidc.o(i.drv_vidc_set_parameter) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_vidc.o(i.drv_vidc_set_parameter) refers to drv_vidc.o(.conststring) for .conststring
    irq_redirect .o(i.ADC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.AP_NRESET_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.DMA_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT0_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT1_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT2_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT3_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT4_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT5_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT6_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT7_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.FLSCTRL_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.HardFault_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.I2C0_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.I2C1_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.LCDC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.MEMC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.MIPI_RX_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.MIPI_TX_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.PWMDET_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SPIM_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SPIS_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SWIRE_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SysTick_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER0_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER1_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER2_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER3_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.UART_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.VIDC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.VPRE_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.WDG_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.handle_init) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.handle_init) refers to drv_common.o(i.app_SysTick_Handler) for app_SysTick_Handler
    irq_redirect .o(i.handle_init) refers to hal_internal_vsync.o(i.app_VIDC_IRQn_Handler) for app_VIDC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) for app_LCDC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler) for app_MIPI_RX_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler) for app_MIPI_TX_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_memc.o(i.app_MEMC_IRQn_Handler) for app_MEMC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to hal_internal_vsync.o(i.app_VPRE_IRQn_Handler) for app_VPRE_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to norflash.o(i.app_fls_ctrl_Handler) for app_fls_ctrl_Handler
    irq_redirect .o(i.handle_init) refers to drv_dma.o(i.app_dma_irq_handler) for app_dma_irq_handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER0_IRQn_Handler) for app_TIMER0_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER1_IRQn_Handler) for app_TIMER1_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER2_IRQn_Handler) for app_TIMER2_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER3_IRQn_Handler) for app_TIMER3_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_wdg.o(i.app_WDG_IRQn_Handler) for app_WDG_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_uart.o(i.app_UART_IRQn_Handler) for app_UART_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_i2c_slave.o(i.app_I2C0_IRQn_Handler) for app_I2C0_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_i2c_master.o(i.app_I2C1_IRQn_Handler) for app_I2C1_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to hal_spi_slave.o(i.app_SPIS_IRQn_Handler) for app_SPIS_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_spi_master.o(i.app_SPIM_IRQn_Handler) for app_SPIM_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_pwm.o(i.app_PWMDET_IRQn_Handler) for app_PWMDET_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_swire.o(i.app_SWIRE_IRQn_Handler) for app_SWIRE_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) for app_AP_NRESET_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler) for app_EXTI_INT0_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler) for app_EXTI_INT1_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler) for app_EXTI_INT2_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler) for app_EXTI_INT3_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler) for app_EXTI_INT4_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler) for app_EXTI_INT5_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler) for app_EXTI_INT6_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler) for app_EXTI_INT7_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_common.o(i.app_HardFault_Handler) for app_HardFault_Handler
    drv_chip_info.o(i.drv_chip_info_get_version) refers to drv_chip_info.o(.data) for .data
    drv_chip_info.o(i.drv_chip_info_init) refers to drv_chip_info.o(.data) for .data
    drv_chip_info.o(i.drv_chip_rx_info_check) refers to printfa.o(i.__0printf) for __2printf
    drv_chip_info.o(i.drv_chip_rx_info_check) refers to drv_chip_info.o(.data) for .data
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to drv_chip_info.o(i.drv_chip_info_get_version) for drv_chip_info_get_version
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to printfa.o(i.__0printf) for __2printf
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to hal_spi_slave.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_s_set_high_impedance) refers to drv_spi_slave.o(i.drv_spi_s_enable) for drv_spi_s_enable
    hal_spi_slave.o(i.hal_spi_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_spi_slave.o(i.hal_spi_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    hal_spi_slave.o(i.hal_spi_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_abort) refers to drv_spi_dma.o(i.drv_spi_abort_dma) for drv_spi_abort_dma
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start) refers to drv_dma.o(i.drv_dma_enable_cycle) for drv_dma_enable_cycle
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start) refers to drv_spi_dma.o(i.drv_spis_dma_write) for drv_spis_dma_write
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_deinit) refers to drv_spi_slave.o(i.drv_spi_s_deinit) for drv_spi_s_deinit
    hal_spi_slave.o(i.hal_spi_slave_disable) refers to drv_spi_slave.o(i.drv_spi_s_enable) for drv_spi_s_enable
    hal_spi_slave.o(i.hal_spi_slave_enable) refers to drv_spi_slave.o(i.drv_spi_s_enable_int) for drv_spi_s_enable_int
    hal_spi_slave.o(i.hal_spi_slave_enable) refers to drv_spi_slave.o(i.drv_spi_s_enable) for drv_spi_s_enable
    hal_spi_slave.o(i.hal_spi_slave_enable) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_spi_slave.o(i.hal_spi_slave_enable) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_gpio_init) refers to drv_spi_slave.o(i.drv_spi_s_gpio_init) for drv_spi_s_gpio_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to hal_spi_slave.o(i.hal_spi_slave_gpio_init) for hal_spi_slave_gpio_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_slave.o(i.drv_spi_slave_init) for drv_spi_slave_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_dma.o(i.drv_spi_dma_init) for drv_spi_dma_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) for drv_spi_set_dma_irq_callback
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_slave.o(i.drv_spi_s_enable_tx_dma) for drv_spi_s_enable_tx_dma
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    hal_spi_slave.o(i.hal_spi_slave_init) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_register_callback) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_reset_tx) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_set_auto_rx_buffer) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_set_auto_tx_buffer) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_write_data) refers to drv_spi_slave.o(i.drv_spi_s_write_data) for drv_spi_s_write_data
    drv_fls_dma.o(i.fls_abort_dma) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_fls_dma.o(i.fls_abort_dma) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls_dma.o(i.fls_dma_rw_prepare) for fls_dma_rw_prepare
    drv_fls_dma.o(i.fls_dma_rw_prepare) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls_dma.o(i.fls_dma_rw_prepare) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls_dma.o(i.fls_dma_rw_prepare) refers to drv_fls.o(i.fls_set_write) for fls_set_write
    drv_fls_dma.o(i.fls_dma_rw_prepare) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls_dma.o(i.fls_dma_rw_prepare) refers to drv_fls_dma.o(i.fls_dma_enable) for fls_dma_enable
    drv_fls_dma.o(i.fls_dma_rw_prepare) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls_dma.o(i.fls_dma_rw_prepare) for fls_dma_rw_prepare
    drv_fls_dma.o(i.fls_read_dmacallback) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to memseta.o(.text) for __aeabi_memclr4
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_fls_dma.o(.data) for .data
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_fls_dma.o(i.fls_read_dmacallback) for fls_read_dmacallback
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_fls_dma.o(i.fls_write_dmacallback) for fls_write_dmacallback
    drv_fls_dma.o(i.fls_transfer_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_fls_dma.o(i.fls_transfer_dma) refers to drv_dma.o(i.drv_dma_start_transfer) for drv_dma_start_transfer
    drv_fls_dma.o(i.fls_transfer_get_receive_count_dma) refers to drv_dma.o(i.drv_dma_get_remaining_bytes) for drv_dma_get_remaining_bytes
    drv_fls_dma.o(i.fls_write_dmacallback) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_pwm.o(i.app_PWMDET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_pwm.o(i.app_PWMDET_IRQn_Handler) refers to drv_pwm.o(.data) for .data
    drv_pwm.o(i.drv_pwm_in_register_callback) refers to drv_pwm.o(.data) for .data
    drv_pwm.o(i.drv_pwm_in_set_sys_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.UART_AbortReceive) refers to drv_uart.o(i.UART_Disable_IT) for UART_Disable_IT
    drv_uart.o(i.UART_AbortReceive) refers to drv_uart.o(i.UART_ResetRxFIFO) for UART_ResetRxFIFO
    drv_uart.o(i.UART_AbortSend) refers to drv_uart.o(i.UART_Disable_IT) for UART_Disable_IT
    drv_uart.o(i.UART_AbortSend) refers to drv_uart.o(i.UART_ResetTxFIFO) for UART_ResetTxFIFO
    drv_uart.o(i.UART_Deinit) refers to drv_uart.o(i.UART_SwitchSCLK) for UART_SwitchSCLK
    drv_uart.o(i.UART_Disable_IT) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_Disable_IT) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.UART_Disable_IT) refers to drv_uart.o(.constdata) for .constdata
    drv_uart.o(i.UART_EnableDma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req) for drv_sys_cfg_set_dma_rx_req
    drv_uart.o(i.UART_EnableDma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    drv_uart.o(i.UART_Enable_IT) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_Enable_IT) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.UART_GetDefaultConfig) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.UART_GetDefaultConfig) refers to drv_common.o(.data) for g_system_clock
    drv_uart.o(i.UART_GetFIFO_Ctrl) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_GetFIFO_Ctrl) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_IRQ_Handle) refers to drv_uart.o(i.UART_TransferHandleIRQ) for UART_TransferHandleIRQ
    drv_uart.o(i.UART_IRQ_Handle) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_uart.o(i.UART_IRQ_Handle) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_ResetRxFIFO) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_ResetRxFIFO) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_ResetTxFIFO) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_ResetTxFIFO) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_SetBaudRate) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_uart.o(i.UART_SwitchSCLK) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_uart.o(i.UART_TransferCreateHandle) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_TransferCreateHandle) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.UART_TransferCreateHandle) refers to drv_uart.o(i.UART_Enable_IT) for UART_Enable_IT
    drv_uart.o(i.UART_TransferCreateHandle) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_TransferHandleIRQ) refers to drv_uart.o(i.UART_ResetRxFIFO) for UART_ResetRxFIFO
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_DisableDma) for UART_DisableDma
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_SwitchSCLK) for UART_SwitchSCLK
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_SetBaudRate) for UART_SetBaudRate
    drv_uart.o(i.UART_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.UART_init) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.app_UART_IRQn_Handler) refers to drv_uart.o(i.UART_IRQ_Handle) for UART_IRQ_Handle
    drv_uart_dma.o(i.UART_DMAInit) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart_dma.o(i.UART_DMAInit) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    drv_uart_dma.o(i.UART_TransferAbortReceiveDMA) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_uart_dma.o(i.UART_TransferAbortSendDMA) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart.o(i.UART_EnableDma) for UART_EnableDma
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(i.UART_DMAInit) for UART_DMAInit
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(.data) for .data
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(i.UART_TransferReceiveDMACallback) for UART_TransferReceiveDMACallback
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(i.UART_TransferSendDMACallback) for UART_TransferSendDMACallback
    drv_uart_dma.o(i.UART_TransferGetReceiveCountDMA) refers to drv_dma.o(i.drv_dma_get_remaining_bytes) for drv_dma_get_remaining_bytes
    drv_uart_dma.o(i.UART_TransferReceiveDMA) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_uart_dma.o(i.UART_TransferReceiveDMA) refers to drv_uart.o(i.UART_EnableDma) for UART_EnableDma
    drv_uart_dma.o(i.UART_TransferReceiveDMA) refers to drv_dma.o(i.drv_dma_start_transfer) for drv_dma_start_transfer
    drv_uart_dma.o(i.UART_TransferSendDMA) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_uart_dma.o(i.UART_TransferSendDMA) refers to drv_uart.o(i.UART_EnableDma) for UART_EnableDma
    drv_uart_dma.o(i.UART_TransferSendDMA) refers to drv_dma.o(i.drv_dma_start_transfer) for drv_dma_start_transfer
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_set_int) for drv_wdg_set_int
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_clear_counter) for drv_wdg_clear_counter
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_read_edge_flag) for drv_wdg_read_edge_flag
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_clear_edge_flag) for drv_wdg_clear_edge_flag
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(.data) for .data
    drv_wdg.o(i.drv_wdg_register_callback) refers to drv_wdg.o(.data) for .data
    drv_wdg.o(i.drv_wdg_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_wdg.o(i.drv_wdg_set_repeat) refers to drv_wdg.o(.data) for .data
    drv_spi_slave.o(i.drv_spi_s_disable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_spi_slave.o(i.drv_spi_s_disable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_spi_slave.o(i.drv_spi_s_enable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_spi_slave.o(i.drv_spi_s_set_intr_callback) refers to drv_spi_slave.o(.data) for .data
    ceil.o(i.__softfp_ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.__softfp_ceil) refers to ceil.o(i.ceil) for ceil
    ceil.o(i.ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.ceil) refers to dadd.o(.text) for __aeabi_dadd
    ceil.o(i.ceil) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry10a.o(.ARM.Collect$$$$0000000D) for __rt_final_cpp
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry11a.o(.ARM.Collect$$$$0000000F) for __rt_final_exit
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry7b.o(.ARM.Collect$$$$00000008) for _main_clock
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry8b.o(.ARM.Collect$$$$0000000A) for _main_cpp_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry9a.o(.ARM.Collect$$$$0000000B) for _main_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry5.o(.ARM.Collect$$$$00000004) for _main_scatterload
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry2.o(.ARM.Collect$$$$00000001) for _main_stk
    idiv.o(.text) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfb.o(i.__0fprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0fprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0printf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printfb.o(i.__0vfprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vfprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printf0.o(i.__0fprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0fprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0printf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf0.o(i.__0vfprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vfprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf1.o(i.__0fprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0fprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0printf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i.__0vfprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vfprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf2.o(i.__0fprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0fprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0printf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf2.o(i.__0vfprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vfprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf3.o(i.__0fprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0fprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0printf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i.__0vfprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vfprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf4.o(i.__0fprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0fprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0printf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i.__0vfprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vfprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf5.o(i.__0fprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0fprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0printf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i.__0vfprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vfprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf6.o(i.__0fprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0fprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0printf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i.__0vfprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vfprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i._printf_core) refers to printf6.o(i._printf_pre_padding) for _printf_pre_padding
    printf6.o(i._printf_core) refers to printf6.o(i._printf_post_padding) for _printf_post_padding
    printf6.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf7.o(i.__0fprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0fprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0printf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i.__0vfprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vfprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i._printf_core) refers to printf7.o(i._printf_pre_padding) for _printf_pre_padding
    printf7.o(i._printf_core) refers to printf7.o(i._printf_post_padding) for _printf_post_padding
    printf7.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf8.o(i.__0fprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0fprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0printf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i.__0vfprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vfprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i._printf_core) refers to printf8.o(i._printf_pre_padding) for _printf_pre_padding
    printf8.o(i._printf_core) refers to printf8.o(i._printf_post_padding) for _printf_post_padding
    printf8.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i.__0fprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0fprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0fprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0printf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0printf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0snprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0snprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0snprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0sprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0sprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0sprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i.__0vfprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vfprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vfprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0vsnprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0vsprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i._fp_digits) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._fp_digits) refers to dmul.o(.text) for __aeabi_dmul
    printfa.o(i._fp_digits) refers to ddiv.o(.text) for __aeabi_ddiv
    printfa.o(i._fp_digits) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    printfa.o(i._fp_digits) refers to dadd.o(.text) for __aeabi_dadd
    printfa.o(i._fp_digits) refers to dfixul.o(.text) for __aeabi_d2ulz
    printfa.o(i._fp_digits) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_core) refers to printfa.o(i._printf_pre_padding) for _printf_pre_padding
    printfa.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers to printfa.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i._printf_core) refers to printfa.o(i._fp_digits) for _fp_digits
    printfa.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfa.o(i._printf_post_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_pre_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._snputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._sputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    fmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers to fepilogue.o(.text) for _float_round
    fscalb.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    dadd.o(.text) refers to llsshr.o(.text) for __aeabi_lasr
    dadd.o(.text) refers to depilogue.o(.text) for _double_epilogue
    fflti.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fflti.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    ffltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ffltui.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    dfltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfltui.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ffixi.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ffixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixi.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixi.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixui.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    f2d.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    cfrcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    entry2.o(.ARM.Collect$$$$00000001) refers to entry2.o(.ARM.Collect$$$$00002712) for __lit__00000000
    entry2.o(.ARM.Collect$$$$00002712) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    entry5.o(.ARM.Collect$$$$00000004) refers to init.o(.text) for __scatterload
    entry9a.o(.ARM.Collect$$$$0000000B) refers to main.o(i.main) for main
    entry9b.o(.ARM.Collect$$$$0000000C) refers to main.o(i.main) for main
    uldiv.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    uldiv.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to depilogue.o(i.__ARM_clz) for __ARM_clz
    depilogue.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dmul.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ddiv.o(.text) refers to depilogue.o(.text) for _double_round
    dfixul.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixul.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    init.o(.text) refers to entry5.o(.ARM.Collect$$$$00000004) for __main_after_scatterload


==============================================================================

Removing Unused input sections from the image.

    Removing main.o(.rev16_text), (4 bytes).
    Removing main.o(.revsh_text), (4 bytes).
    Removing ap_demo.o(.rev16_text), (4 bytes).
    Removing ap_demo.o(.revsh_text), (4 bytes).
    Removing ap_demo.o(.data), (1 bytes).
    Removing ap_demo.o(.data), (4 bytes).
    Removing app_tp_for_custom_s8.o(.rev16_text), (4 bytes).
    Removing app_tp_for_custom_s8.o(.revsh_text), (4 bytes).
    Removing app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const), (56 bytes).
    Removing app_tp_for_custom_s8.o(.bss), (200 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (37 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (1 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (3 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (3 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (11 bytes).
    Removing app_tp_for_custom_s8.o(.data), (10 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (64 bytes).
    Removing app_tp_for_custom_s8.o(.data), (3 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (32 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_transfer.o(.rev16_text), (4 bytes).
    Removing app_tp_transfer.o(.revsh_text), (4 bytes).
    Removing app_tp_transfer.o(i.app_tp_phone_reset_on), (12 bytes).
    Removing app_tp_transfer.o(i.app_tp_s_transfer_complate), (26 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (5 bytes).
    Removing app_tp_transfer.o(.data), (6 bytes).
    Removing app_tp_transfer.o(.data), (2 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (1 bytes).
    Removing app_tp_transfer.o(.data), (2 bytes).
    Removing app_tp_transfer.o(.data), (2 bytes).
    Removing board.o(.rev16_text), (4 bytes).
    Removing board.o(.revsh_text), (4 bytes).
    Removing startup_armcm0.o(HEAP), (3072 bytes).
    Removing hal_dsi_rx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd), (88 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_short_cmd), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern), (296 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en), (16 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode), (128 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle), (32 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart), (72 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk), (44 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_pq_enh_chr), (56 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_pq_enh_chr2), (64 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_pq_enh_lum), (56 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_pq_gain), (64 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter), (120 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_dcs_direct_mode), (8 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter), (40 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format), (56 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk), (64 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_te_waveform), (52 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex), (14 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate), (112 bytes).
    Removing hal_dsi_tx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic), (164 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_ulps_mode), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_ulps_mode), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd), (140 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle), (28 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_pq_edge), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_pq_filter), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_horizon_flip), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_lp_cmd), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg), (24 bytes).
    Removing hal_gpio.o(.rev16_text), (4 bytes).
    Removing hal_gpio.o(.revsh_text), (4 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_int_type), (20 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_pull_state), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_driving_strength), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_output_data_ex), (36 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_schmitt_trigger), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_slew_rate), (32 bytes).
    Removing hal_i2c_master.o(.rev16_text), (4 bytes).
    Removing hal_i2c_master.o(.revsh_text), (4 bytes).
    Removing hal_i2c_master.o(i.hal_i2c_m_deinit), (8 bytes).
    Removing hal_i2c_master.o(i.hal_i2c_m_set_high_impedance), (46 bytes).
    Removing hal_i2c_slave.o(.rev16_text), (4 bytes).
    Removing hal_i2c_slave.o(.revsh_text), (4 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_deinit), (8 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_get_tx_byte_num), (8 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_read_complate), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_read_complate_clear), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_read_data), (8 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_rxfifo_notempty), (16 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_set_dma_tx_cycle), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance), (46 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_write_complate), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_write_data), (8 bytes).
    Removing hal_spi_master.o(.rev16_text), (4 bytes).
    Removing hal_spi_master.o(.revsh_text), (4 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_callback), (28 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_deinit), (10 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_dma_init), (64 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_dma_read), (64 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_dma_write), (40 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_get_transfer_complate), (36 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_gpio_init), (8 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_set_high_impedance), (94 bytes).
    Removing hal_spi_master.o(.data), (1 bytes).
    Removing hal_swire.o(.rev16_text), (4 bytes).
    Removing hal_swire.o(.revsh_text), (4 bytes).
    Removing hal_swire.o(i.hal_swire_deinit), (18 bytes).
    Removing hal_swire.o(i.hal_swire_init), (32 bytes).
    Removing hal_swire.o(i.hal_swire_register_callback), (10 bytes).
    Removing hal_swire.o(i.hal_swire_start), (112 bytes).
    Removing hal_system.o(.rev16_text), (4 bytes).
    Removing hal_system.o(.revsh_text), (4 bytes).
    Removing hal_system.o(i.hal_system_deep_sleep_mode), (8 bytes).
    Removing hal_system.o(i.hal_system_disable_systick), (8 bytes).
    Removing hal_system.o(i.hal_system_flash_read), (56 bytes).
    Removing hal_system.o(i.hal_system_flash_write), (58 bytes).
    Removing hal_system.o(i.hal_system_get_tick), (8 bytes).
    Removing hal_system.o(i.hal_system_idle_mode), (8 bytes).
    Removing hal_system.o(i.hal_system_register_systick_cb), (8 bytes).
    Removing hal_system.o(i.hal_system_reset_chip), (32 bytes).
    Removing hal_system.o(i.hal_system_share_flash_mode), (20 bytes).
    Removing hal_system.o(i.hal_system_sleep_mode), (48 bytes).
    Removing hal_timer.o(.rev16_text), (4 bytes).
    Removing hal_timer.o(.revsh_text), (4 bytes).
    Removing hal_timer.o(i.hal_timer_deinit), (46 bytes).
    Removing hal_timer.o(i.hal_timer_get_status), (8 bytes).
    Removing hal_timer.o(i.hal_timer_set_repeat), (8 bytes).
    Removing hal_timer.o(i.hal_timer_start_ex), (72 bytes).
    Removing tau_delay.o(.rev16_text), (4 bytes).
    Removing tau_delay.o(.revsh_text), (4 bytes).
    Removing tau_log.o(.rev16_text), (4 bytes).
    Removing tau_log.o(.revsh_text), (4 bytes).
    Removing tau_log.o(i.fgetc), (22 bytes).
    Removing norflash.o(.rev16_text), (4 bytes).
    Removing norflash.o(.revsh_text), (4 bytes).
    Removing norflash.o(i.norflash_best_cfg_init), (44 bytes).
    Removing norflash.o(i.norflash_big_end_clear), (14 bytes).
    Removing norflash.o(i.norflash_big_end_enable), (20 bytes).
    Removing norflash.o(i.norflash_check_crc32), (14 bytes).
    Removing norflash.o(i.norflash_check_id), (72 bytes).
    Removing norflash.o(i.norflash_dma_callback), (24 bytes).
    Removing norflash.o(i.norflash_dma_read), (148 bytes).
    Removing norflash.o(i.norflash_dma_write), (244 bytes).
    Removing norflash.o(i.norflash_dual_read), (60 bytes).
    Removing norflash.o(i.norflash_dual_write), (112 bytes).
    Removing norflash.o(i.norflash_en4b), (40 bytes).
    Removing norflash.o(i.norflash_en_quad), (116 bytes).
    Removing norflash.o(i.norflash_en_quad_check), (64 bytes).
    Removing norflash.o(i.norflash_erase_block), (44 bytes).
    Removing norflash.o(i.norflash_erase_chip), (28 bytes).
    Removing norflash.o(i.norflash_erase_sector), (44 bytes).
    Removing norflash.o(i.norflash_ex4b), (40 bytes).
    Removing norflash.o(i.norflash_exit_quad), (76 bytes).
    Removing norflash.o(i.norflash_get_dual_hstatus), (52 bytes).
    Removing norflash.o(i.norflash_get_hstatus), (52 bytes).
    Removing norflash.o(i.norflash_get_status), (52 bytes).
    Removing norflash.o(i.norflash_init), (48 bytes).
    Removing norflash.o(i.norflash_quad_read), (76 bytes).
    Removing norflash.o(i.norflash_quad_write), (108 bytes).
    Removing norflash.o(i.norflash_read), (28 bytes).
    Removing norflash.o(i.norflash_read_config_reg), (36 bytes).
    Removing norflash.o(i.norflash_read_id), (20 bytes).
    Removing norflash.o(i.norflash_reset), (2 bytes).
    Removing norflash.o(i.norflash_reset_crc32), (32 bytes).
    Removing norflash.o(i.norflash_set_best_cfg), (50 bytes).
    Removing norflash.o(i.norflash_set_best_read_cfg), (84 bytes).
    Removing norflash.o(i.norflash_set_best_write_cfg), (84 bytes).
    Removing norflash.o(i.norflash_switch_fls_spi), (112 bytes).
    Removing norflash.o(i.norflash_write), (96 bytes).
    Removing norflash.o(i.norflash_write_disable), (64 bytes).
    Removing norflash.o(i.norflash_write_enable), (56 bytes).
    Removing norflash.o(i.norflash_write_endian_scr), (132 bytes).
    Removing norflash.o(.bss), (116 bytes).
    Removing norflash.o(.bss), (32 bytes).
    Removing norflash.o(.data), (2 bytes).
    Removing hal_uart.o(.rev16_text), (4 bytes).
    Removing hal_uart.o(.revsh_text), (4 bytes).
    Removing hal_uart.o(i.hal_uart_deinit), (20 bytes).
    Removing hal_uart.o(i.hal_uart_dmacallback), (36 bytes).
    Removing hal_uart.o(i.hal_uart_receive_blocking), (16 bytes).
    Removing hal_uart.o(i.hal_uart_receive_dma), (72 bytes).
    Removing hal_uart.o(i.hal_uart_transmit_dma), (68 bytes).
    Removing drv_common.o(.rev16_text), (4 bytes).
    Removing drv_common.o(.revsh_text), (4 bytes).
    Removing drv_common.o(i.drv_common_disable_systick), (20 bytes).
    Removing drv_common.o(i.drv_common_get_otp_value), (28 bytes).
    Removing drv_common.o(i.drv_common_get_tick), (12 bytes).
    Removing drv_common.o(i.drv_common_idle_mode), (40 bytes).
    Removing drv_common.o(i.drv_common_systick_register_cb), (12 bytes).
    Removing drv_crgu.o(.rev16_text), (4 bytes).
    Removing drv_crgu.o(.revsh_text), (4 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_all_reset_flags), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_reset_flag), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_config_clocks), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_config_clocks_div), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_config_clocks_src), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_ana_clk_status), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_fpga_id), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_mipi_ref_src), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_reset_flag), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_system_clk), (28 bytes).
    Removing drv_crgu.o(i.drv_crgu_reset_chip), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_200m_scan_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_300m_scan_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_abp_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_adc_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_adc_src), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_fls_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_fls_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_monitor_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_monitor_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_swire_div), (20 bytes).
    Removing drv_dma.o(.rev16_text), (4 bytes).
    Removing drv_dma.o(.revsh_text), (4 bytes).
    Removing drv_dma.o(i.drv_dma_abort_transfer), (18 bytes).
    Removing drv_dma.o(i.drv_dma_ahb_init), (72 bytes).
    Removing drv_dma.o(i.drv_dma_channel_is_active), (28 bytes).
    Removing drv_dma.o(i.drv_dma_deinit), (32 bytes).
    Removing drv_dma.o(i.drv_dma_disenable_channel_interrupts), (32 bytes).
    Removing drv_dma.o(i.drv_dma_get_remaining_bytes), (36 bytes).
    Removing drv_dma.o(i.drv_dma_init), (20 bytes).
    Removing drv_dma.o(i.drv_dma_m2m_init), (66 bytes).
    Removing drv_dma.o(i.drv_dma_reset), (10 bytes).
    Removing drv_dma.o(i.drv_dma_set_ccr), (114 bytes).
    Removing drv_dma.o(i.drv_dma_start_transfer), (18 bytes).
    Removing drv_fls.o(.rev16_text), (4 bytes).
    Removing drv_fls.o(.revsh_text), (4 bytes).
    Removing drv_fls.o(i.__NVIC_DisableIRQ), (32 bytes).
    Removing drv_fls.o(i.drv_fls_gpio_connect), (28 bytes).
    Removing drv_fls.o(i.drv_fls_gpio_disconnect), (32 bytes).
    Removing drv_fls.o(i.fls_EnableClk), (12 bytes).
    Removing drv_fls.o(i.fls_busy_pending), (12 bytes).
    Removing drv_fls.o(i.fls_ctrl_cfg_init), (72 bytes).
    Removing drv_fls.o(i.fls_ddat_enable), (24 bytes).
    Removing drv_fls.o(i.fls_de_init), (44 bytes).
    Removing drv_fls.o(i.fls_descr), (10 bytes).
    Removing drv_fls.o(i.fls_disable_it), (36 bytes).
    Removing drv_fls.o(i.fls_en_scr), (10 bytes).
    Removing drv_fls.o(i.fls_enable_it), (48 bytes).
    Removing drv_fls.o(i.fls_get_crcout), (4 bytes).
    Removing drv_fls.o(i.fls_get_default_fls_config), (20 bytes).
    Removing drv_fls.o(i.fls_get_default_spi_config), (44 bytes).
    Removing drv_fls.o(i.fls_get_default_tuning), (12 bytes).
    Removing drv_fls.o(i.fls_get_tuning), (18 bytes).
    Removing drv_fls.o(i.fls_init), (62 bytes).
    Removing drv_fls.o(i.fls_qadr_enable), (22 bytes).
    Removing drv_fls.o(i.fls_qcmd_enable), (22 bytes).
    Removing drv_fls.o(i.fls_qdat_enable), (22 bytes).
    Removing drv_fls.o(i.fls_read_byte_data), (126 bytes).
    Removing drv_fls.o(i.fls_read_cmd), (104 bytes).
    Removing drv_fls.o(i.fls_read_cmd_it), (110 bytes).
    Removing drv_fls.o(i.fls_reset_crc), (18 bytes).
    Removing drv_fls.o(i.fls_scr_clear), (10 bytes).
    Removing drv_fls.o(i.fls_set_addr_dummy), (32 bytes).
    Removing drv_fls.o(i.fls_set_addr_len), (32 bytes).
    Removing drv_fls.o(i.fls_set_irq_mask), (26 bytes).
    Removing drv_fls.o(i.fls_set_read), (10 bytes).
    Removing drv_fls.o(i.fls_set_tuning), (24 bytes).
    Removing drv_fls.o(i.fls_set_write), (10 bytes).
    Removing drv_fls.o(i.fls_single_mode), (16 bytes).
    Removing drv_fls.o(i.fls_spi_init), (180 bytes).
    Removing drv_fls.o(i.fls_spi_start), (10 bytes).
    Removing drv_fls.o(i.fls_swrst), (18 bytes).
    Removing drv_fls.o(i.fls_write_byte_data), (160 bytes).
    Removing drv_fls.o(i.fls_write_cmd), (58 bytes).
    Removing drv_fls.o(.data), (4 bytes).
    Removing drv_gpio.o(.rev16_text), (4 bytes).
    Removing drv_gpio.o(.revsh_text), (4 bytes).
    Removing drv_gpio.o(i.drv_gpio_get_pull_state), (224 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_driving_strength), (312 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_schmitt_trigger), (168 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_slew_rate), (168 bytes).
    Removing drv_i2c_dma.o(.rev16_text), (4 bytes).
    Removing drv_i2c_dma.o(.revsh_text), (4 bytes).
    Removing drv_i2c_master.o(.rev16_text), (4 bytes).
    Removing drv_i2c_master.o(.revsh_text), (4 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_bus_init), (36 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_deinit), (44 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_enable), (32 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_get_fifo_status), (28 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_read_data), (32 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_set_fifo_threshold), (24 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_set_sys_mask), (48 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_write_data), (32 bytes).
    Removing drv_i2c_slave.o(.rev16_text), (4 bytes).
    Removing drv_i2c_slave.o(.revsh_text), (4 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_bus_init), (36 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_deinit), (44 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_enable), (32 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_get_tx_byte_num), (12 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_read_data), (32 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_set_fifo_threshold), (24 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_set_sys_mask), (48 bytes).
    Removing drv_param_init.o(.rev16_text), (4 bytes).
    Removing drv_param_init.o(.revsh_text), (4 bytes).
    Removing drv_param_init.o(i.drv_param_init_set_scld_filter), (100 bytes).
    Removing drv_param_init.o(i.drv_param_init_set_sclu_filter), (52 bytes).
    Removing drv_param_init.o(i.drv_param_set_enh_chr), (12 bytes).
    Removing drv_param_init.o(i.drv_param_set_enh_chr2), (16 bytes).
    Removing drv_param_init.o(i.drv_param_set_enh_lum), (12 bytes).
    Removing drv_param_init.o(i.drv_param_set_gain), (16 bytes).
    Removing drv_param_init.o(.data), (4 bytes).
    Removing drv_param_init.o(.data), (4 bytes).
    Removing drv_param_init.o(.data), (4 bytes).
    Removing drv_param_init.o(.data), (4 bytes).
    Removing drv_param_init.o(.data), (4 bytes).
    Removing drv_param_init.o(.data), (4 bytes).
    Removing drv_param_init.o(.data), (4 bytes).
    Removing drv_param_init.o(.data), (4 bytes).
    Removing drv_param_init.o(.data), (4 bytes).
    Removing drv_param_init.o(.data), (4 bytes).
    Removing drv_pwr.o(.rev16_text), (4 bytes).
    Removing drv_pwr.o(.revsh_text), (4 bytes).
    Removing drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode), (40 bytes).
    Removing drv_spi_dma.o(.rev16_text), (4 bytes).
    Removing drv_spi_dma.o(.revsh_text), (4 bytes).
    Removing drv_spi_dma.o(i.__NVIC_ClearPendingIRQ), (24 bytes).
    Removing drv_spi_dma.o(i.drv_spi_abort_dma), (80 bytes).
    Removing drv_spi_dma.o(i.drv_spi_dma_callback), (52 bytes).
    Removing drv_spi_dma.o(i.drv_spi_dma_init), (188 bytes).
    Removing drv_spi_dma.o(i.drv_spi_set_dma_irq_callback), (80 bytes).
    Removing drv_spi_dma.o(i.drv_spim_dma_read), (512 bytes).
    Removing drv_spi_dma.o(i.drv_spim_dma_write), (84 bytes).
    Removing drv_spi_dma.o(i.drv_spis_dma_write), (56 bytes).
    Removing drv_spi_dma.o(.bss), (24 bytes).
    Removing drv_spi_dma.o(.data), (8 bytes).
    Removing drv_spi_master.o(.rev16_text), (4 bytes).
    Removing drv_spi_master.o(.revsh_text), (4 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_deinit), (56 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_disable_int), (72 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_enable), (32 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_enable_int), (76 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_enable_rx_dma), (32 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_enable_tx_dma), (28 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_gpio_init), (32 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_set_intr_callback), (12 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_write_data), (44 bytes).
    Removing drv_spi_master.o(i.drv_spi_master_init), (164 bytes).
    Removing drv_swire.o(.rev16_text), (4 bytes).
    Removing drv_swire.o(.revsh_text), (4 bytes).
    Removing drv_swire.o(i.drv_swire_enable), (28 bytes).
    Removing drv_swire.o(i.drv_swire_register_callback), (12 bytes).
    Removing drv_swire.o(i.drv_swire_set_bit_time), (24 bytes).
    Removing drv_swire.o(i.drv_swire_set_pulse_count), (12 bytes).
    Removing drv_sys_cfg.o(.rev16_text), (4 bytes).
    Removing drv_sys_cfg.o(.revsh_text), (4 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_dma_req_mask), (32 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_read_version0_id), (12 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_set_ap_reset), (28 bytes).
    Removing drv_timer.o(.rev16_text), (4 bytes).
    Removing drv_timer.o(.revsh_text), (4 bytes).
    Removing drv_timer.o(i.drv_timer_get_status), (38 bytes).
    Removing drv_timer.o(i.drv_timer_set_repeat), (16 bytes).
    Removing dcs_packet_fifo.o(i.dcs_packet_get_fifo_size), (16 bytes).
    Removing hal_internal_vsync.o(.rev16_text), (4 bytes).
    Removing hal_internal_vsync.o(.revsh_text), (4 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode), (48 bytes).
    Removing drv_dsi_rx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_rx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate), (66 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_version), (4 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration), (236 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg), (32 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg), (48 bytes).
    Removing drv_dsi_rx.o(i.drv_rx_phy_test_read), (12 bytes).
    Removing drv_dsi_tx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_tx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_force_interrupt), (8 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_get_phy_status), (6 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_forcepll), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration), (232 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_start), (18 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock), (10 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot), (62 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger), (92 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter), (344 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit), (276 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_sdf_3d), (28 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_bta), (22 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_vpg), (70 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_version), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_vid_shadow), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_read), (10 bytes).
    Removing drv_lcdc.o(.rev16_text), (4 bytes).
    Removing drv_lcdc.o(.revsh_text), (4 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_config_rgb_to_pentile), (26 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_config_sclu_filter), (54 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_enable), (42 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_disp_buff_pix), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_read_buff_data), (40 bytes).
    Removing drv_memc.o(.rev16_text), (4 bytes).
    Removing drv_memc.o(.revsh_text), (4 bytes).
    Removing drv_memc.o(i.drv_memc_set_ahb2ram), (14 bytes).
    Removing drv_memc.o(i.drv_memc_set_fb_pri_inverse), (16 bytes).
    Removing drv_memc.o(i.drv_memc_set_inten), (20 bytes).
    Removing drv_phy_common.o(.rev16_text), (4 bytes).
    Removing drv_phy_common.o(.revsh_text), (4 bytes).
    Removing drv_phy_common.o(i.drv_phy_test_read), (8 bytes).
    Removing drv_rxbr.o(.rev16_text), (4 bytes).
    Removing drv_rxbr.o(.revsh_text), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_dsc_flush), (16 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_err_reset), (98 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_ipi_vsync_interval), (8 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_pix_fmt), (8 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg), (10 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_hw_rcv_cmd), (8 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_col_addr), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_compress), (24 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_page_addr), (4 bytes).
    Removing drv_vidc.o(.rev16_text), (4 bytes).
    Removing drv_vidc.o(.revsh_text), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_clear_status0), (14 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_cap_pixel), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_signal_frame), (30 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_irq_status), (18 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status0), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status1), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status2), (6 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_dsc_thresh), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_frmst_latency), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_inff_thresh), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_outff_thresh), (14 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_parameter), (576 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_pentile_swap), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_y4t2_hinit), (14 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_y4t2_vinit), (14 bytes).
    Removing drv_vidc.o(i.drv_vidc_update_src_format), (14 bytes).
    Removing drv_vidc.o(.conststring), (344 bytes).
    Removing irq_redirect .o(.rev16_text), (4 bytes).
    Removing irq_redirect .o(.revsh_text), (4 bytes).
    Removing drv_chip_info.o(.rev16_text), (4 bytes).
    Removing drv_chip_info.o(.revsh_text), (4 bytes).
    Removing drv_dsc_dec.o(.rev16_text), (4 bytes).
    Removing drv_dsc_dec.o(.revsh_text), (4 bytes).
    Removing drv_dsc_dec.o(i.drv_dsc_dec_set_u32_pps), (120 bytes).
    Removing hal_spi_slave.o(.rev16_text), (4 bytes).
    Removing hal_spi_slave.o(.revsh_text), (4 bytes).
    Removing hal_spi_slave.o(i.hal_spi_s_set_high_impedance), (94 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_auto_transfer_abort), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start), (52 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_busy), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_deinit), (10 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_disable), (12 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_enable), (96 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_flush_fifo), (28 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_get_rxfifo_notempty), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_gpio_init), (8 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_init), (76 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_read_data), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_register_callback), (12 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_reset_tx), (68 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_set_auto_rx_buffer), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_set_auto_tx_buffer), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_write_data), (14 bytes).
    Removing drv_fls_dma.o(.rev16_text), (4 bytes).
    Removing drv_fls_dma.o(.revsh_text), (4 bytes).
    Removing drv_fls_dma.o(i.fls_abort_dma), (42 bytes).
    Removing drv_fls_dma.o(i.fls_dma_disable), (10 bytes).
    Removing drv_fls_dma.o(i.fls_dma_enable), (10 bytes).
    Removing drv_fls_dma.o(i.fls_dma_read_prepare), (22 bytes).
    Removing drv_fls_dma.o(i.fls_dma_rw_prepare), (100 bytes).
    Removing drv_fls_dma.o(i.fls_dma_write_prepare), (22 bytes).
    Removing drv_fls_dma.o(i.fls_read_dmacallback), (36 bytes).
    Removing drv_fls_dma.o(i.fls_transfer_create_handle_dma), (188 bytes).
    Removing drv_fls_dma.o(i.fls_transfer_dma), (102 bytes).
    Removing drv_fls_dma.o(i.fls_transfer_get_receive_count_dma), (34 bytes).
    Removing drv_fls_dma.o(i.fls_write_dmacallback), (36 bytes).
    Removing drv_fls_dma.o(.data), (8 bytes).
    Removing drv_pwm.o(.rev16_text), (4 bytes).
    Removing drv_pwm.o(.revsh_text), (4 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_clear_pwm_int_all), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_enable), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_counter_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_current_count), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_high_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_low_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_register_callback), (24 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_set_pwm_int), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_set_sys_int), (52 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_enable), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_get_sync_flag), (16 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_pause), (28 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_control), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_sync_mode), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_threshold), (12 bytes).
    Removing drv_uart.o(.rev16_text), (4 bytes).
    Removing drv_uart.o(.revsh_text), (4 bytes).
    Removing drv_uart.o(i.UART_AbortReceive), (30 bytes).
    Removing drv_uart.o(i.UART_AbortSend), (30 bytes).
    Removing drv_uart.o(i.UART_Deinit), (28 bytes).
    Removing drv_uart.o(i.UART_Disable_IT), (68 bytes).
    Removing drv_uart.o(i.UART_EnableDma), (32 bytes).
    Removing drv_uart.o(i.UART_Enable_IT), (44 bytes).
    Removing drv_uart.o(i.UART_GetDefaultConfig), (72 bytes).
    Removing drv_uart.o(i.UART_GetFIFO_Ctrl), (20 bytes).
    Removing drv_uart.o(i.UART_GetReceiveCount), (22 bytes).
    Removing drv_uart.o(i.UART_GetReceiveStatus), (20 bytes).
    Removing drv_uart.o(i.UART_GetRxRingBufferLength), (28 bytes).
    Removing drv_uart.o(i.UART_GetSendCount), (22 bytes).
    Removing drv_uart.o(i.UART_GetSendStatus), (20 bytes).
    Removing drv_uart.o(i.UART_ReadBlocking), (32 bytes).
    Removing drv_uart.o(i.UART_ReceiveNonBlocking), (50 bytes).
    Removing drv_uart.o(i.UART_ResetTxFIFO), (36 bytes).
    Removing drv_uart.o(i.UART_SendNonBlocking), (38 bytes).
    Removing drv_uart.o(i.UART_TransferCreateHandle), (96 bytes).
    Removing drv_uart.o(i.UART_TransferStartRingBuffer), (30 bytes).
    Removing drv_uart.o(.constdata), (1 bytes).
    Removing drv_uart_dma.o(.rev16_text), (4 bytes).
    Removing drv_uart_dma.o(.revsh_text), (4 bytes).
    Removing drv_uart_dma.o(i.UART_DMAInit), (70 bytes).
    Removing drv_uart_dma.o(i.UART_TransferAbortReceiveDMA), (16 bytes).
    Removing drv_uart_dma.o(i.UART_TransferAbortSendDMA), (16 bytes).
    Removing drv_uart_dma.o(i.UART_TransferCreateHandleDMA), (168 bytes).
    Removing drv_uart_dma.o(i.UART_TransferGetReceiveCountDMA), (34 bytes).
    Removing drv_uart_dma.o(i.UART_TransferReceiveDMA), (54 bytes).
    Removing drv_uart_dma.o(i.UART_TransferReceiveDMACallback), (38 bytes).
    Removing drv_uart_dma.o(i.UART_TransferSendDMA), (54 bytes).
    Removing drv_uart_dma.o(i.UART_TransferSendDMACallback), (38 bytes).
    Removing drv_uart_dma.o(.data), (8 bytes).
    Removing drv_wdg.o(.rev16_text), (4 bytes).
    Removing drv_wdg.o(.revsh_text), (4 bytes).
    Removing drv_wdg.o(i.drv_wdg_enable), (32 bytes).
    Removing drv_wdg.o(i.drv_wdg_load_match), (12 bytes).
    Removing drv_wdg.o(i.drv_wdg_register_callback), (12 bytes).
    Removing drv_wdg.o(i.drv_wdg_sel_mode), (28 bytes).
    Removing drv_wdg.o(i.drv_wdg_set_repeat), (12 bytes).
    Removing drv_spi_slave.o(.rev16_text), (4 bytes).
    Removing drv_spi_slave.o(.revsh_text), (4 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_deinit), (52 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_disable_int), (64 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_enable), (32 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_enable_int), (72 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_enable_rx_dma), (32 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_enable_tx_dma), (28 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_gpio_init), (24 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_read_data), (32 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_set_intr_callback), (12 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_write_data), (44 bytes).
    Removing drv_spi_slave.o(i.drv_spi_slave_init), (76 bytes).
    Removing drv_spi_slave.o(.data), (4 bytes).

570 unused section(s) (total 22786 bytes) removed from the image.

==============================================================================

Image Symbol Table

    Local Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    ../clib/../cmprslib/zerorunl2.c          0x00000000   Number         0  __dczerorl2.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uldiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  idiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uidiv.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry5.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry2.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11b.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llshl.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llushr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llsshr.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf7.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf6.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf5.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf4.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf2.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf1.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf0.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfb.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf3.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfa.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf8.o ABSOLUTE
    ../clib/microlib/printf/stubs.s          0x00000000   Number         0  stubs.o ABSOLUTE
    ../clib/microlib/stdio/streams.c         0x00000000   Number         0  stdout.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpyb.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpya.o ABSOLUTE
    ../clib/microlib/string/memset.c         0x00000000   Number         0  memseta.o ABSOLUTE
    ../clib/microlib/stubs.s                 0x00000000   Number         0  iusefp.o ABSOLUTE
    ../fplib/microlib/f2d.c                  0x00000000   Number         0  f2d.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  fadd.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  dadd.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  fdiv.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  ddiv.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  depilogue.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  fepilogue.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  ffixi.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  ffixui.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixui.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixul.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixi.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  ffltui.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  dfltui.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  fflti.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  fmul.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  dmul.o ABSOLUTE
    ../fplib/microlib/fpscalb.c              0x00000000   Number         0  fscalb.o ABSOLUTE
    ../mathlib/ceil.c                        0x00000000   Number         0  ceil.o ABSOLUTE
    ..\..\..\src\common\tau_delay.c          0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\..\..\src\common\tau_log.c            0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\..\..\src\driver\lark\src\drv_chip_info.c 0x00000000   Number         0  drv_chip_info.o ABSOLUTE
    ..\..\..\src\driver\lark\src\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\..\..\src\driver\source\lark\drv\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\..\..\src\driver\source\lark\drv\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\..\..\src\driver\source\lark\drv\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\..\..\src\driver\source\lark\drv\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\..\..\src\driver\source\lark\drv\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\..\..\src\driver\source\lark\drv\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\..\..\src\driver\source\lark\drv\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\..\..\src\driver\source\lark\drv\irq_redirect .c 0x00000000   Number         0  irq_redirect .o ABSOLUTE
    ..\..\..\src\driver\source\lark\hal\internal\dcs_packet_fifo.c 0x00000000   Number         0  dcs_packet_fifo.o ABSOLUTE
    ..\..\..\src\driver\source\lark\hal\internal\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\drv\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\drv\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\drv\drv_dma.c  0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\drv\drv_fls.c  0x00000000   Number         0  drv_fls.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\drv\drv_fls_dma.c 0x00000000   Number         0  drv_fls_dma.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\drv\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\drv\drv_i2c_dma.c 0x00000000   Number         0  drv_i2c_dma.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\drv\drv_i2c_master.c 0x00000000   Number         0  drv_i2c_master.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\drv\drv_i2c_slave.c 0x00000000   Number         0  drv_i2c_slave.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\drv\drv_param_init.c 0x00000000   Number         0  drv_param_init.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\drv\drv_pwm.c  0x00000000   Number         0  drv_pwm.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\drv\drv_pwr.c  0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\drv\drv_spi_dma.c 0x00000000   Number         0  drv_spi_dma.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\drv\drv_spi_master.c 0x00000000   Number         0  drv_spi_master.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\drv\drv_spi_slave.c 0x00000000   Number         0  drv_spi_slave.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\drv\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\drv\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\drv\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\drv\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\drv\drv_uart_dma.c 0x00000000   Number         0  drv_uart_dma.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\drv\drv_wdg.c  0x00000000   Number         0  drv_wdg.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\hal\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\hal\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\hal\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\hal\hal_i2c_master.c 0x00000000   Number         0  hal_i2c_master.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\hal\hal_i2c_slave.c 0x00000000   Number         0  hal_i2c_slave.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\hal\hal_spi_master.c 0x00000000   Number         0  hal_spi_master.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\hal\hal_spi_slave.c 0x00000000   Number         0  hal_spi_slave.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\hal\hal_swire.c 0x00000000   Number         0  hal_swire.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\hal\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\hal\hal_timer.c 0x00000000   Number         0  hal_timer.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\hal\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\..\..\src\sdk\lark\src\hal\internal\norflash.c 0x00000000   Number         0  norflash.o ABSOLUTE
    ..\..\src\app\demo\ap_demo.c             0x00000000   Number         0  ap_demo.o ABSOLUTE
    ..\..\src\app\demo\app_tp_for_custom_s8.c 0x00000000   Number         0  app_tp_for_custom_s8.o ABSOLUTE
    ..\..\src\app\demo\app_tp_transfer.c     0x00000000   Number         0  app_tp_transfer.o ABSOLUTE
    ..\..\src\app\main.c                     0x00000000   Number         0  main.o ABSOLUTE
    ..\..\src\board\board.c                  0x00000000   Number         0  board.o ABSOLUTE
    ..\..\src\board\startup\startup_ARMCM0.s 0x00000000   Number         0  startup_armcm0.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_delay.c     0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_log.c       0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\\..\\..\\src\\driver\\lark\\src\\drv_chip_info.c 0x00000000   Number         0  drv_chip_info.o ABSOLUTE
    ..\\..\\..\\src\\driver\\lark\\src\\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\lark\\drv\\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\lark\\drv\\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\lark\\drv\\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\lark\\drv\\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\lark\\drv\\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\lark\\drv\\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\lark\\drv\\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\lark\\drv\\irq_redirect .c 0x00000000   Number         0  irq_redirect .o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\lark\\hal\\internal\\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\drv\\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\drv\\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\drv\\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\drv\\drv_fls.c 0x00000000   Number         0  drv_fls.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\drv\\drv_fls_dma.c 0x00000000   Number         0  drv_fls_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\drv\\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\drv\\drv_i2c_dma.c 0x00000000   Number         0  drv_i2c_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\drv\\drv_i2c_master.c 0x00000000   Number         0  drv_i2c_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\drv\\drv_i2c_slave.c 0x00000000   Number         0  drv_i2c_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\drv\\drv_param_init.c 0x00000000   Number         0  drv_param_init.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\drv\\drv_pwm.c 0x00000000   Number         0  drv_pwm.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\drv\\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\drv\\drv_spi_dma.c 0x00000000   Number         0  drv_spi_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\drv\\drv_spi_master.c 0x00000000   Number         0  drv_spi_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\drv\\drv_spi_slave.c 0x00000000   Number         0  drv_spi_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\drv\\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\drv\\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\drv\\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\drv\\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\drv\\drv_uart_dma.c 0x00000000   Number         0  drv_uart_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\drv\\drv_wdg.c 0x00000000   Number         0  drv_wdg.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\hal\\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\hal\\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\hal\\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\hal\\hal_i2c_master.c 0x00000000   Number         0  hal_i2c_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\hal\\hal_i2c_slave.c 0x00000000   Number         0  hal_i2c_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\hal\\hal_spi_master.c 0x00000000   Number         0  hal_spi_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\hal\\hal_spi_slave.c 0x00000000   Number         0  hal_spi_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\hal\\hal_swire.c 0x00000000   Number         0  hal_swire.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\hal\\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\hal\\hal_timer.c 0x00000000   Number         0  hal_timer.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\hal\\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\lark\\src\\hal\\internal\\norflash.c 0x00000000   Number         0  norflash.o ABSOLUTE
    ..\\..\\src\\app\\demo\\ap_demo.c        0x00000000   Number         0  ap_demo.o ABSOLUTE
    ..\\..\\src\\app\\demo\\app_tp_for_custom_s8.c 0x00000000   Number         0  app_tp_for_custom_s8.o ABSOLUTE
    ..\\..\\src\\app\\demo\\app_tp_transfer.c 0x00000000   Number         0  app_tp_transfer.o ABSOLUTE
    ..\\..\\src\\app\\main.c                 0x00000000   Number         0  main.o ABSOLUTE
    ..\\..\\src\\board\\board.c              0x00000000   Number         0  board.o ABSOLUTE
    cdrcmple.s                               0x00000000   Number         0  cdrcmple.o ABSOLUTE
    cfrcmple.s                               0x00000000   Number         0  cfrcmple.o ABSOLUTE
    dc.s                                     0x00000000   Number         0  dc.o ABSOLUTE
    handlers.s                               0x00000000   Number         0  handlers.o ABSOLUTE
    init.s                                   0x00000000   Number         0  init.o ABSOLUTE
    RESET                                    0x00010000   Section      192  startup_armcm0.o(RESET)
    .ARM.Collect$$$$00000000                 0x000100c0   Section        0  entry.o(.ARM.Collect$$$$00000000)
    .ARM.Collect$$$$00000001                 0x000100c0   Section        4  entry2.o(.ARM.Collect$$$$00000001)
    .ARM.Collect$$$$00000004                 0x000100c4   Section        4  entry5.o(.ARM.Collect$$$$00000004)
    .ARM.Collect$$$$00000008                 0x000100c8   Section        0  entry7b.o(.ARM.Collect$$$$00000008)
    .ARM.Collect$$$$0000000A                 0x000100c8   Section        0  entry8b.o(.ARM.Collect$$$$0000000A)
    .ARM.Collect$$$$0000000B                 0x000100c8   Section        8  entry9a.o(.ARM.Collect$$$$0000000B)
    .ARM.Collect$$$$0000000D                 0x000100d0   Section        0  entry10a.o(.ARM.Collect$$$$0000000D)
    .ARM.Collect$$$$0000000F                 0x000100d0   Section        0  entry11a.o(.ARM.Collect$$$$0000000F)
    .ARM.Collect$$$$00002712                 0x000100d0   Section        4  entry2.o(.ARM.Collect$$$$00002712)
    __lit__00000000                          0x000100d0   Data           4  entry2.o(.ARM.Collect$$$$00002712)
    .text                                    0x000100d4   Section      120  startup_armcm0.o(.text)
    .text                                    0x0001014c   Section        0  uidiv.o(.text)
    .text                                    0x00010178   Section        0  idiv.o(.text)
    .text                                    0x000101a0   Section        0  memcpya.o(.text)
    .text                                    0x000101c4   Section        0  memseta.o(.text)
    .text                                    0x000101e8   Section        0  fadd.o(.text)
    .text                                    0x0001029a   Section        0  fmul.o(.text)
    .text                                    0x00010314   Section        0  fdiv.o(.text)
    .text                                    0x00010390   Section        0  fscalb.o(.text)
    .text                                    0x000103a8   Section        0  dadd.o(.text)
    .text                                    0x0001050c   Section        0  fflti.o(.text)
    .text                                    0x00010522   Section        0  ffltui.o(.text)
    .text                                    0x00010530   Section        0  dfltui.o(.text)
    .text                                    0x0001054c   Section        0  ffixi.o(.text)
    .text                                    0x0001057e   Section        0  ffixui.o(.text)
    .text                                    0x000105a8   Section        0  dfixi.o(.text)
    .text                                    0x000105f0   Section        0  dfixui.o(.text)
    .text                                    0x0001062c   Section        0  f2d.o(.text)
    .text                                    0x00010654   Section       20  cfrcmple.o(.text)
    .text                                    0x00010668   Section        0  uldiv.o(.text)
    .text                                    0x000106c8   Section        0  llshl.o(.text)
    .text                                    0x000106e8   Section        0  llushr.o(.text)
    .text                                    0x0001070a   Section        0  llsshr.o(.text)
    .text                                    0x00010730   Section        0  fepilogue.o(.text)
    .text                                    0x00010730   Section        0  iusefp.o(.text)
    .text                                    0x000107b2   Section        0  depilogue.o(.text)
    .text                                    0x00010870   Section        0  dmul.o(.text)
    .text                                    0x00010940   Section        0  ddiv.o(.text)
    .text                                    0x00010a30   Section        0  dfixul.o(.text)
    .text                                    0x00010a70   Section       40  cdrcmple.o(.text)
    .text                                    0x00010a98   Section       36  init.o(.text)
    .text                                    0x00010abc   Section        0  __dczerorl2.o(.text)
    i.ADC_IRQn_Handler                       0x00010b14   Section        0  irq_redirect .o(i.ADC_IRQn_Handler)
    i.AP_NRESET_IRQn_Handler                 0x00010b2c   Section        0  irq_redirect .o(i.AP_NRESET_IRQn_Handler)
    i.DMA_IRQn_Handler                       0x00010b48   Section        0  irq_redirect .o(i.DMA_IRQn_Handler)
    i.EXTI_INT0_IRQn_Handler                 0x00010b5c   Section        0  irq_redirect .o(i.EXTI_INT0_IRQn_Handler)
    i.EXTI_INT1_IRQn_Handler                 0x00010b78   Section        0  irq_redirect .o(i.EXTI_INT1_IRQn_Handler)
    i.EXTI_INT2_IRQn_Handler                 0x00010b94   Section        0  irq_redirect .o(i.EXTI_INT2_IRQn_Handler)
    i.EXTI_INT3_IRQn_Handler                 0x00010bb0   Section        0  irq_redirect .o(i.EXTI_INT3_IRQn_Handler)
    i.EXTI_INT4_IRQn_Handler                 0x00010bcc   Section        0  irq_redirect .o(i.EXTI_INT4_IRQn_Handler)
    i.EXTI_INT5_IRQn_Handler                 0x00010be8   Section        0  irq_redirect .o(i.EXTI_INT5_IRQn_Handler)
    i.EXTI_INT6_IRQn_Handler                 0x00010c04   Section        0  irq_redirect .o(i.EXTI_INT6_IRQn_Handler)
    i.EXTI_INT7_IRQn_Handler                 0x00010c20   Section        0  irq_redirect .o(i.EXTI_INT7_IRQn_Handler)
    i.FLSCTRL_IRQn_Handler                   0x00010c3c   Section        0  irq_redirect .o(i.FLSCTRL_IRQn_Handler)
    i.Gpio_swire_output                      0x00010c50   Section        0  ap_demo.o(i.Gpio_swire_output)
    i.HardFault_Handler                      0x00010cc4   Section        0  irq_redirect .o(i.HardFault_Handler)
    i.I2C0_IRQn_Handler                      0x00010cd8   Section        0  irq_redirect .o(i.I2C0_IRQn_Handler)
    i.I2C1_IRQn_Handler                      0x00010cf0   Section        0  irq_redirect .o(i.I2C1_IRQn_Handler)
    i.LCDC_IRQn_Handler                      0x00010d08   Section        0  irq_redirect .o(i.LCDC_IRQn_Handler)
    i.LOG_printf                             0x00010d20   Section        0  tau_log.o(i.LOG_printf)
    i.MEMC_IRQn_Handler                      0x00010d48   Section        0  irq_redirect .o(i.MEMC_IRQn_Handler)
    i.MIPI_RX_IRQn_Handler                   0x00010d60   Section        0  irq_redirect .o(i.MIPI_RX_IRQn_Handler)
    i.MIPI_TX_IRQn_Handler                   0x00010d78   Section        0  irq_redirect .o(i.MIPI_TX_IRQn_Handler)
    i.PWMDET_IRQn_Handler                    0x00010d90   Section        0  irq_redirect .o(i.PWMDET_IRQn_Handler)
    i.S20_Start_init                         0x00010dac   Section        0  app_tp_transfer.o(i.S20_Start_init)
    i.SPIM_IRQn_Handler                      0x00010ed0   Section        0  irq_redirect .o(i.SPIM_IRQn_Handler)
    i.SPIS_IRQn_Handler                      0x00010eec   Section        0  irq_redirect .o(i.SPIS_IRQn_Handler)
    i.SWIRE_IRQn_Handler                     0x00010f08   Section        0  irq_redirect .o(i.SWIRE_IRQn_Handler)
    i.SysTick_Handler                        0x00010f24   Section        0  irq_redirect .o(i.SysTick_Handler)
    i.TIMER0_IRQn_Handler                    0x00010f3c   Section        0  irq_redirect .o(i.TIMER0_IRQn_Handler)
    i.TIMER1_IRQn_Handler                    0x00010f54   Section        0  irq_redirect .o(i.TIMER1_IRQn_Handler)
    i.TIMER2_IRQn_Handler                    0x00010f6c   Section        0  irq_redirect .o(i.TIMER2_IRQn_Handler)
    i.TIMER3_IRQn_Handler                    0x00010f84   Section        0  irq_redirect .o(i.TIMER3_IRQn_Handler)
    i.UART_DisableDma                        0x00010f9c   Section        0  drv_uart.o(i.UART_DisableDma)
    i.UART_GetInstance                       0x00010f9e   Section        0  drv_uart.o(i.UART_GetInstance)
    i.UART_IRQ_Handle                        0x00010fa4   Section        0  drv_uart.o(i.UART_IRQ_Handle)
    i.UART_IRQn_Handler                      0x00010fc0   Section        0  irq_redirect .o(i.UART_IRQn_Handler)
    i.UART_ResetRxFIFO                       0x00010fd8   Section        0  drv_uart.o(i.UART_ResetRxFIFO)
    i.__scatterload_null                     0x00010ffc   Section        2  handlers.o(i.__scatterload_null)
    .constdata                               0x00010ffe   Section        1  app_tp_for_custom_s8.o(.constdata)
    .ARM.__at_0x11000                        0x00011000   Section       20  drv_common.o(.ARM.__at_0x11000)
    i.UART_SetBaudRate                       0x00011014   Section        0  drv_uart.o(i.UART_SetBaudRate)
    i.UART_SwitchSCLK                        0x0001105c   Section        0  drv_uart.o(i.UART_SwitchSCLK)
    i.UART_TransferHandleIRQ                 0x00011076   Section        0  drv_uart.o(i.UART_TransferHandleIRQ)
    i.UART_WriteBlocking                     0x000111aa   Section        0  drv_uart.o(i.UART_WriteBlocking)
    i.UART_init                              0x000111c4   Section        0  drv_uart.o(i.UART_init)
    i.VIDC_IRQn_Handler                      0x00011280   Section        0  irq_redirect .o(i.VIDC_IRQn_Handler)
    i.VPRE_IRQn_Handler                      0x00011298   Section        0  irq_redirect .o(i.VPRE_IRQn_Handler)
    i.WDG_IRQn_Handler                       0x000112b0   Section        0  irq_redirect .o(i.WDG_IRQn_Handler)
    i.__0printf                              0x000112c8   Section        0  printfa.o(i.__0printf)
    i.__0vsprintf                            0x000112e8   Section        0  printfa.o(i.__0vsprintf)
    i.__ARM_clz                              0x0001130c   Section        0  depilogue.o(i.__ARM_clz)
    i.__ARM_common_switch8                   0x0001133a   Section        0  ap_demo.o(i.__ARM_common_switch8)
    i.__NVIC_ClearPendingIRQ                 0x00011354   Section        0  drv_i2c_master.o(i.__NVIC_ClearPendingIRQ)
    __NVIC_ClearPendingIRQ                   0x00011355   Thumb Code    18  drv_i2c_master.o(i.__NVIC_ClearPendingIRQ)
    i.__NVIC_ClearPendingIRQ                 0x0001136c   Section        0  drv_i2c_slave.o(i.__NVIC_ClearPendingIRQ)
    __NVIC_ClearPendingIRQ                   0x0001136d   Thumb Code    18  drv_i2c_slave.o(i.__NVIC_ClearPendingIRQ)
    i.__NVIC_SetPriority                     0x00011384   Section        0  hal_spi_slave.o(i.__NVIC_SetPriority)
    __NVIC_SetPriority                       0x00011385   Thumb Code    60  hal_spi_slave.o(i.__NVIC_SetPriority)
    i.__scatterload_copy                     0x000113c8   Section       14  handlers.o(i.__scatterload_copy)
    i.__scatterload_zeroinit                 0x000113d6   Section       14  handlers.o(i.__scatterload_zeroinit)
    i._fp_digits                             0x000113e4   Section        0  printfa.o(i._fp_digits)
    _fp_digits                               0x000113e5   Thumb Code   344  printfa.o(i._fp_digits)
    i._printf_core                           0x00011558   Section        0  printfa.o(i._printf_core)
    _printf_core                             0x00011559   Thumb Code  1754  printfa.o(i._printf_core)
    i._printf_post_padding                   0x00011c44   Section        0  printfa.o(i._printf_post_padding)
    _printf_post_padding                     0x00011c45   Thumb Code    32  printfa.o(i._printf_post_padding)
    i._printf_pre_padding                    0x00011c64   Section        0  printfa.o(i._printf_pre_padding)
    _printf_pre_padding                      0x00011c65   Thumb Code    44  printfa.o(i._printf_pre_padding)
    i._sputc                                 0x00011c90   Section        0  printfa.o(i._sputc)
    _sputc                                   0x00011c91   Thumb Code    10  printfa.o(i._sputc)
    i.ap_dcs_read                            0x00011c9c   Section        0  ap_demo.o(i.ap_dcs_read)
    ap_dcs_read                              0x00011c9d   Thumb Code  5006  ap_demo.o(i.ap_dcs_read)
    i.ap_demo                                0x00013030   Section        0  ap_demo.o(i.ap_demo)
    i.ap_get_reg_ca                          0x000131a4   Section        0  ap_demo.o(i.ap_get_reg_ca)
    ap_get_reg_ca                            0x000131a5   Thumb Code    38  ap_demo.o(i.ap_get_reg_ca)
    i.ap_get_reg_df                          0x000131d0   Section        0  ap_demo.o(i.ap_get_reg_df)
    ap_get_reg_df                            0x000131d1   Thumb Code   172  ap_demo.o(i.ap_get_reg_df)
    i.ap_reset_cb                            0x00013280   Section        0  ap_demo.o(i.ap_reset_cb)
    ap_reset_cb                              0x00013281   Thumb Code    40  ap_demo.o(i.ap_reset_cb)
    i.ap_set_backlight                       0x000132dc   Section        0  ap_demo.o(i.ap_set_backlight)
    ap_set_backlight                         0x000132dd   Thumb Code   832  ap_demo.o(i.ap_set_backlight)
    i.ap_set_display_off                     0x0001363c   Section        0  ap_demo.o(i.ap_set_display_off)
    ap_set_display_off                       0x0001363d   Thumb Code    42  ap_demo.o(i.ap_set_display_off)
    i.ap_set_display_on                      0x00013694   Section        0  ap_demo.o(i.ap_set_display_on)
    ap_set_display_on                        0x00013695   Thumb Code    22  ap_demo.o(i.ap_set_display_on)
    i.ap_set_enter_sleep_mode                0x000136d8   Section        0  ap_demo.o(i.ap_set_enter_sleep_mode)
    ap_set_enter_sleep_mode                  0x000136d9   Thumb Code    42  ap_demo.o(i.ap_set_enter_sleep_mode)
    i.ap_set_exit_sleep_mode                 0x00013738   Section        0  ap_demo.o(i.ap_set_exit_sleep_mode)
    ap_set_exit_sleep_mode                   0x00013739   Thumb Code    20  ap_demo.o(i.ap_set_exit_sleep_mode)
    i.ap_set_tp_calibration_04               0x00013780   Section        0  ap_demo.o(i.ap_set_tp_calibration_04)
    ap_set_tp_calibration_04                 0x00013781   Thumb Code    22  ap_demo.o(i.ap_set_tp_calibration_04)
    i.ap_tp_calibration                      0x0001379c   Section        0  app_tp_transfer.o(i.ap_tp_calibration)
    i.ap_tp_scan_point_init                  0x0001384c   Section        0  app_tp_transfer.o(i.ap_tp_scan_point_init)
    i.ap_tp_scan_point_record_event          0x00013868   Section        0  app_tp_transfer.o(i.ap_tp_scan_point_record_event)
    i.ap_tp_scan_point_record_event_exec     0x00013904   Section        0  app_tp_transfer.o(i.ap_tp_scan_point_record_event_exec)
    i.ap_tp_simulate_finger_release_event    0x00013954   Section        0  app_tp_transfer.o(i.ap_tp_simulate_finger_release_event)
    i.ap_tp_system_softReset                 0x00013988   Section        0  app_tp_transfer.o(i.ap_tp_system_softReset)
    i.app_AP_NRESET_IRQn_Handler             0x000139c8   Section        0  drv_gpio.o(i.app_AP_NRESET_IRQn_Handler)
    i.app_EXTI_INT0_IRQn_Handler             0x000139ec   Section        0  drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler)
    i.app_EXTI_INT1_IRQn_Handler             0x00013a08   Section        0  drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler)
    i.app_EXTI_INT2_IRQn_Handler             0x00013a24   Section        0  drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler)
    i.app_EXTI_INT3_IRQn_Handler             0x00013a40   Section        0  drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler)
    i.app_EXTI_INT4_IRQn_Handler             0x00013a5c   Section        0  drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler)
    i.app_EXTI_INT5_IRQn_Handler             0x00013a78   Section        0  drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler)
    i.app_EXTI_INT6_IRQn_Handler             0x00013a94   Section        0  drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler)
    i.app_EXTI_INT7_IRQn_Handler             0x00013ab0   Section        0  drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler)
    i.app_HardFault_Handler                  0x00013acc   Section        0  drv_common.o(i.app_HardFault_Handler)
    i.app_I2C0_IRQn_Handler                  0x00013b14   Section        0  drv_i2c_slave.o(i.app_I2C0_IRQn_Handler)
    i.app_I2C1_IRQn_Handler                  0x00013b24   Section        0  drv_i2c_master.o(i.app_I2C1_IRQn_Handler)
    i.app_LCDC_IRQn_Handler                  0x00013b34   Section        0  hal_internal_vsync.o(i.app_LCDC_IRQn_Handler)
    i.app_MEMC_IRQn_Handler                  0x00013c14   Section        0  drv_memc.o(i.app_MEMC_IRQn_Handler)
    i.app_MIPI_RX_IRQn_Handler               0x00013c74   Section        0  drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler)
    i.app_MIPI_TX_IRQn_Handler               0x00013f0c   Section        0  drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler)
    i.app_PWMDET_IRQn_Handler                0x00013fac   Section        0  drv_pwm.o(i.app_PWMDET_IRQn_Handler)
    i.app_SPIM_IRQn_Handler                  0x00013ff4   Section        0  drv_spi_master.o(i.app_SPIM_IRQn_Handler)
    i.app_SPIS_IRQn_Handler                  0x00014014   Section        0  hal_spi_slave.o(i.app_SPIS_IRQn_Handler)
    i.app_SWIRE_IRQn_Handler                 0x00014214   Section        0  drv_swire.o(i.app_SWIRE_IRQn_Handler)
    i.app_SysTick_Handler                    0x00014234   Section        0  drv_common.o(i.app_SysTick_Handler)
    i.app_TIMER0_IRQn_Handler                0x0001424c   Section        0  drv_timer.o(i.app_TIMER0_IRQn_Handler)
    i.app_TIMER1_IRQn_Handler                0x00014256   Section        0  drv_timer.o(i.app_TIMER1_IRQn_Handler)
    i.app_TIMER2_IRQn_Handler                0x00014260   Section        0  drv_timer.o(i.app_TIMER2_IRQn_Handler)
    i.app_TIMER3_IRQn_Handler                0x0001426a   Section        0  drv_timer.o(i.app_TIMER3_IRQn_Handler)
    i.app_UART_IRQn_Handler                  0x00014274   Section        0  drv_uart.o(i.app_UART_IRQn_Handler)
    i.app_VIDC_IRQn_Handler                  0x0001427c   Section        0  hal_internal_vsync.o(i.app_VIDC_IRQn_Handler)
    i.app_VPRE_IRQn_Handler                  0x00014360   Section        0  hal_internal_vsync.o(i.app_VPRE_IRQn_Handler)
    i.app_WDG_IRQn_Handler                   0x000145e4   Section        0  drv_wdg.o(i.app_WDG_IRQn_Handler)
    i.app_dma_irq_handler                    0x0001461c   Section        0  drv_dma.o(i.app_dma_irq_handler)
    i.app_fls_ctrl_Handler                   0x00014624   Section        0  norflash.o(i.app_fls_ctrl_Handler)
    i.app_tp_I2C_init                        0x00014654   Section        0  app_tp_transfer.o(i.app_tp_I2C_init)
    i.app_tp_calibration_exec                0x00014678   Section        0  ap_demo.o(i.app_tp_calibration_exec)
    i.app_tp_i2cs_callback                   0x000146d4   Section        0  app_tp_transfer.o(i.app_tp_i2cs_callback)
    app_tp_i2cs_callback                     0x000146d5   Thumb Code    10  app_tp_transfer.o(i.app_tp_i2cs_callback)
    i.app_tp_init                            0x000146e0   Section        0  app_tp_transfer.o(i.app_tp_init)
    i.app_tp_m_read                          0x00014728   Section        0  app_tp_transfer.o(i.app_tp_m_read)
    app_tp_m_read                            0x00014729   Thumb Code    32  app_tp_transfer.o(i.app_tp_m_read)
    i.app_tp_m_transfer_complate             0x00014748   Section        0  app_tp_transfer.o(i.app_tp_m_transfer_complate)
    i.app_tp_m_write                         0x00014750   Section        0  app_tp_transfer.o(i.app_tp_m_write)
    app_tp_m_write                           0x00014751   Thumb Code     8  app_tp_transfer.o(i.app_tp_m_write)
    i.app_tp_phone_analysis_data             0x00014758   Section        0  app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data)
    i.app_tp_phone_clear_reset_on            0x00014b68   Section        0  app_tp_transfer.o(i.app_tp_phone_clear_reset_on)
    i.app_tp_s_read                          0x00014b74   Section        0  app_tp_transfer.o(i.app_tp_s_read)
    i.app_tp_s_write                         0x00014b7c   Section        0  app_tp_transfer.o(i.app_tp_s_write)
    i.app_tp_screen_analysis_int             0x00014b84   Section        0  app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int)
    i.app_tp_screen_init                     0x00014e50   Section        0  app_tp_transfer.o(i.app_tp_screen_init)
    i.app_tp_screen_int_callback             0x00014e80   Section        0  app_tp_transfer.o(i.app_tp_screen_int_callback)
    app_tp_screen_int_callback               0x00014e81   Thumb Code     8  app_tp_transfer.o(i.app_tp_screen_int_callback)
    i.app_tp_screen_int_init                 0x00014e8c   Section        0  app_tp_transfer.o(i.app_tp_screen_int_init)
    app_tp_screen_int_init                   0x00014e8d   Thumb Code    48  app_tp_transfer.o(i.app_tp_screen_int_init)
    i.app_tp_screen_int_lvl_low              0x00014ec4   Section        0  app_tp_transfer.o(i.app_tp_screen_int_lvl_low)
    app_tp_screen_int_lvl_low                0x00014ec5   Thumb Code     4  app_tp_transfer.o(i.app_tp_screen_int_lvl_low)
    i.app_tp_transfer_phone                  0x00014ec8   Section        0  app_tp_transfer.o(i.app_tp_transfer_phone)
    app_tp_transfer_phone                    0x00014ec9   Thumb Code    44  app_tp_transfer.o(i.app_tp_transfer_phone)
    i.app_tp_transfer_screen_const           0x00014ef8   Section        0  app_tp_transfer.o(i.app_tp_transfer_screen_const)
    app_tp_transfer_screen_const             0x00014ef9   Thumb Code    50  app_tp_transfer.o(i.app_tp_transfer_screen_const)
    i.app_tp_transfer_screen_int             0x00014f38   Section        0  app_tp_transfer.o(i.app_tp_transfer_screen_int)
    i.app_tp_transfer_screen_start           0x00015118   Section        0  app_tp_transfer.o(i.app_tp_transfer_screen_start)
    i.blue_change_ccm                        0x00015130   Section        0  ap_demo.o(i.blue_change_ccm)
    i.board_Init                             0x00015168   Section        0  board.o(i.board_Init)
    i.calc_framebuffer_setting               0x00015184   Section        0  hal_internal_vsync.o(i.calc_framebuffer_setting)
    calc_framebuffer_setting                 0x00015185   Thumb Code   462  hal_internal_vsync.o(i.calc_framebuffer_setting)
    i.ceil                                   0x00015370   Section        0  ceil.o(i.ceil)
    i.check_mipi_rx_tx_video_info            0x00015438   Section        0  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    check_mipi_rx_tx_video_info              0x00015439   Thumb Code    44  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    i.check_pkt_buf_rev                      0x00015464   Section        0  hal_internal_vsync.o(i.check_pkt_buf_rev)
    check_pkt_buf_rev                        0x00015465   Thumb Code    38  hal_internal_vsync.o(i.check_pkt_buf_rev)
    i.dcs_packet_fifo_alloc                  0x00015490   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    i.dcs_packet_fifo_init                   0x000154e8   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    i.dcs_packet_free_fifo_header            0x00015500   Section        0  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    i.dcs_packet_get_fifo_header             0x00015544   Section        0  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    i.dcs_sw_filter                          0x00015568   Section        0  hal_internal_vsync.o(i.dcs_sw_filter)
    dcs_sw_filter                            0x00015569   Thumb Code    24  hal_internal_vsync.o(i.dcs_sw_filter)
    i.delayMs                                0x00015584   Section        0  tau_delay.o(i.delayMs)
    i.delayUs                                0x0001559c   Section        0  tau_delay.o(i.delayUs)
    i.disable_mipi_timer_cb                  0x000155c0   Section        0  ap_demo.o(i.disable_mipi_timer_cb)
    disable_mipi_timer_cb                    0x000155c1   Thumb Code    88  ap_demo.o(i.disable_mipi_timer_cb)
    i.drv_ap_rst_trig_edge_detect            0x00015654   Section        0  drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect)
    i.drv_chip_info_get_version              0x0001568c   Section        0  drv_chip_info.o(i.drv_chip_info_get_version)
    i.drv_chip_info_init                     0x00015698   Section        0  drv_chip_info.o(i.drv_chip_info_init)
    i.drv_chip_rx_info_check                 0x00015748   Section        0  drv_chip_info.o(i.drv_chip_rx_info_check)
    i.drv_chip_rx_init_done                  0x000157a4   Section        0  drv_chip_info.o(i.drv_chip_rx_init_done)
    i.drv_common_enable_systick              0x000157b8   Section        0  drv_common.o(i.drv_common_enable_systick)
    i.drv_common_system_init                 0x00015810   Section        0  drv_common.o(i.drv_common_system_init)
    i.drv_crgu_config_reset_modules          0x00015840   Section        0  drv_crgu.o(i.drv_crgu_config_reset_modules)
    i.drv_crgu_set_ahb_pre_div               0x00015850   Section        0  drv_crgu.o(i.drv_crgu_set_ahb_pre_div)
    i.drv_crgu_set_ahb_src                   0x00015864   Section        0  drv_crgu.o(i.drv_crgu_set_ahb_src)
    i.drv_crgu_set_clock                     0x00015878   Section        0  drv_crgu.o(i.drv_crgu_set_clock)
    i.drv_crgu_set_dpi_mux_src               0x00015898   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_mux_src)
    i.drv_crgu_set_dpi_pre_div               0x000158ac   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_pre_div)
    i.drv_crgu_set_dpi_pre_src               0x000158c4   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_pre_src)
    i.drv_crgu_set_dsc_core_div              0x000158d8   Section        0  drv_crgu.o(i.drv_crgu_set_dsc_core_div)
    i.drv_crgu_set_dsco_src                  0x000158ec   Section        0  drv_crgu.o(i.drv_crgu_set_dsco_src)
    i.drv_crgu_set_dsco_src_div              0x00015900   Section        0  drv_crgu.o(i.drv_crgu_set_dsco_src_div)
    i.drv_crgu_set_fb_div                    0x00015914   Section        0  drv_crgu.o(i.drv_crgu_set_fb_div)
    i.drv_crgu_set_fb_src                    0x00015928   Section        0  drv_crgu.o(i.drv_crgu_set_fb_src)
    i.drv_crgu_set_lcdc_div                  0x0001593c   Section        0  drv_crgu.o(i.drv_crgu_set_lcdc_div)
    i.drv_crgu_set_lcdc_src                  0x00015950   Section        0  drv_crgu.o(i.drv_crgu_set_lcdc_src)
    i.drv_crgu_set_mipi_cfg_src              0x00015964   Section        0  drv_crgu.o(i.drv_crgu_set_mipi_cfg_src)
    i.drv_crgu_set_mipi_ref_src              0x00015978   Section        0  drv_crgu.o(i.drv_crgu_set_mipi_ref_src)
    i.drv_crgu_set_reset                     0x00015990   Section        0  drv_crgu.o(i.drv_crgu_set_reset)
    i.drv_crgu_set_rxbr_div                  0x000159a8   Section        0  drv_crgu.o(i.drv_crgu_set_rxbr_div)
    i.drv_crgu_set_rxbr_src                  0x000159bc   Section        0  drv_crgu.o(i.drv_crgu_set_rxbr_src)
    i.drv_crgu_set_vidc_src                  0x000159d0   Section        0  drv_crgu.o(i.drv_crgu_set_vidc_src)
    i.drv_dma_clear_flag                     0x000159e4   Section        0  drv_dma.o(i.drv_dma_clear_flag)
    i.drv_dma_create_handle                  0x00015a00   Section        0  drv_dma.o(i.drv_dma_create_handle)
    i.drv_dma_disenable_channel              0x00015a18   Section        0  drv_dma.o(i.drv_dma_disenable_channel)
    i.drv_dma_enable_channel                 0x00015a30   Section        0  drv_dma.o(i.drv_dma_enable_channel)
    i.drv_dma_enable_channel_interrupts      0x00015a48   Section        0  drv_dma.o(i.drv_dma_enable_channel_interrupts)
    i.drv_dma_enable_cycle                   0x00015a7c   Section        0  drv_dma.o(i.drv_dma_enable_cycle)
    i.drv_dma_get_channel_flag               0x00015aac   Section        0  drv_dma.o(i.drv_dma_get_channel_flag)
    i.drv_dma_irq_handler                    0x00015ac0   Section        0  drv_dma.o(i.drv_dma_irq_handler)
    i.drv_dma_prepar_transfer                0x00015b3c   Section        0  drv_dma.o(i.drv_dma_prepar_transfer)
    i.drv_dma_set_burst                      0x00015b54   Section        0  drv_dma.o(i.drv_dma_set_burst)
    i.drv_dma_set_callback                   0x00015b70   Section        0  drv_dma.o(i.drv_dma_set_callback)
    i.drv_dma_set_transfer                   0x00015b78   Section        0  drv_dma.o(i.drv_dma_set_transfer)
    i.drv_dsc_dec_convert_pps_rc_parameter   0x00015bbc   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter)
    i.drv_dsc_dec_disable                    0x00015bf2   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    i.drv_dsc_dec_enable                     0x00015c00   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    i.drv_dsc_dec_get_nslc                   0x00015cb4   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    i.drv_dsc_dec_set_u8_pps                 0x00015cbe   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps)
    i.drv_dsi_rx_calc_ipi_tx_delay           0x00015ce8   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    i.drv_dsi_rx_enable_irq                  0x00015dec   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    i.drv_dsi_rx_get_color_bpp               0x00015e2c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    drv_dsi_rx_get_color_bpp                 0x00015e2d   Thumb Code    62  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    i.drv_dsi_rx_get_color_pcc               0x00015e7c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    drv_dsi_rx_get_color_pcc                 0x00015e7d   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    i.drv_dsi_rx_get_compression_en          0x00015e98   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    i.drv_dsi_rx_get_max_ret_size            0x00015ea0   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size)
    i.drv_dsi_rx_power_up                    0x00015ea6   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    i.drv_dsi_rx_set_ctrl_cfg                0x00015eb4   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    i.drv_dsi_rx_set_ddi_cfg                 0x00015ed0   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    i.drv_dsi_rx_set_inten                   0x00015ee0   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    i.drv_dsi_rx_set_ipi_cfg                 0x00015ee4   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    i.drv_dsi_rx_set_resp_cnt                0x00015ef4   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    i.drv_dsi_rx_set_up_phy                  0x00015f1c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    i.drv_dsi_rx_shut_down                   0x00015fac   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    i.drv_dsi_tx_command_header              0x00015fba   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    i.drv_dsi_tx_command_mode_cfg            0x00015fce   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    i.drv_dsi_tx_command_put_payload         0x0001603a   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    i.drv_dsi_tx_config_eotp                 0x0001603e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    i.drv_dsi_tx_config_int                  0x00016056   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    i.drv_dsi_tx_dpi_lpcmd_time              0x0001605e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    i.drv_dsi_tx_dpi_mode                    0x00016066   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    i.drv_dsi_tx_dpi_polarity                0x00016070   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    i.drv_dsi_tx_get_cmd_status              0x00016094   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    i.drv_dsi_tx_mode                        0x00016098   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    i.drv_dsi_tx_phy_clock_lane_auto_lp      0x0001609c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    i.drv_dsi_tx_phy_clock_lane_req_hs       0x000160b4   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    i.drv_dsi_tx_phy_lane_mode               0x000160ce   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    i.drv_dsi_tx_phy_status_ready            0x000160da   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    i.drv_dsi_tx_phy_status_stopstate        0x0001613e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    i.drv_dsi_tx_phy_test_setup              0x0001617c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    i.drv_dsi_tx_phy_time_cfg                0x00016260   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    i.drv_dsi_tx_powerup                     0x0001627e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    i.drv_dsi_tx_response_mode               0x00016286   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    i.drv_dsi_tx_set_bta_ack                 0x000162a2   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    i.drv_dsi_tx_set_esc_div                 0x000162ba   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    i.drv_dsi_tx_set_int                     0x000162c8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    i.drv_dsi_tx_set_time_out_div            0x000162fc   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    i.drv_dsi_tx_set_video_chunk             0x0001630c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    i.drv_dsi_tx_set_video_timing            0x00016314   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    i.drv_dsi_tx_shutdown                    0x00016336   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    i.drv_dsi_tx_timeout_cfg                 0x0001633e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    i.drv_dsi_tx_video_mode_cfg              0x00016364   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    i.drv_dsi_tx_video_mode_disable_hact_cmd 0x0001640e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_disable_hact_cmd)
    i.drv_dsi_tx_video_mode_set_lp_cmd       0x00016424   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd)
    i.drv_gpio_get_input_data                0x0001643c   Section        0  drv_gpio.o(i.drv_gpio_get_input_data)
    i.drv_gpio_register_ap_reset_callback    0x00016454   Section        0  drv_gpio.o(i.drv_gpio_register_ap_reset_callback)
    i.drv_gpio_register_callback             0x00016460   Section        0  drv_gpio.o(i.drv_gpio_register_callback)
    i.drv_gpio_set_int                       0x00016474   Section        0  drv_gpio.o(i.drv_gpio_set_int)
    i.drv_gpio_set_ioe                       0x000164b8   Section        0  drv_gpio.o(i.drv_gpio_set_ioe)
    i.drv_gpio_set_mode0                     0x000164d8   Section        0  drv_gpio.o(i.drv_gpio_set_mode0)
    i.drv_gpio_set_mode1                     0x000164e8   Section        0  drv_gpio.o(i.drv_gpio_set_mode1)
    i.drv_gpio_set_mode2                     0x000164f8   Section        0  drv_gpio.o(i.drv_gpio_set_mode2)
    i.drv_gpio_set_mode3                     0x00016508   Section        0  drv_gpio.o(i.drv_gpio_set_mode3)
    i.drv_gpio_set_output_data               0x00016518   Section        0  hal_gpio.o(i.drv_gpio_set_output_data)
    drv_gpio_set_output_data                 0x00016519   Thumb Code    26  hal_gpio.o(i.drv_gpio_set_output_data)
    i.drv_gpio_set_pull_state                0x00016538   Section        0  drv_gpio.o(i.drv_gpio_set_pull_state)
    i.drv_i2c_clear_m_it_pending_bit         0x00016668   Section        0  drv_i2c_master.o(i.drv_i2c_clear_m_it_pending_bit)
    i.drv_i2c_clear_s_it_pending_bit         0x000166c8   Section        0  drv_i2c_slave.o(i.drv_i2c_clear_s_it_pending_bit)
    i.drv_i2c_dma_callback                   0x00016724   Section        0  drv_i2c_dma.o(i.drv_i2c_dma_callback)
    drv_i2c_dma_callback                     0x00016725   Thumb Code    38  drv_i2c_dma.o(i.drv_i2c_dma_callback)
    i.drv_i2c_dma_init                       0x00016758   Section        0  drv_i2c_dma.o(i.drv_i2c_dma_init)
    i.drv_i2c_enable_rx_dma                  0x00016804   Section        0  drv_i2c_dma.o(i.drv_i2c_enable_rx_dma)
    i.drv_i2c_enable_tx_dma                  0x0001681e   Section        0  drv_i2c_dma.o(i.drv_i2c_enable_tx_dma)
    i.drv_i2c_m_enable_intr                  0x00016838   Section        0  drv_i2c_master.o(i.drv_i2c_m_enable_intr)
    i.drv_i2c_m_set_callback                 0x00016870   Section        0  drv_i2c_master.o(i.drv_i2c_m_set_callback)
    i.drv_i2c_master_init                    0x0001687c   Section        0  drv_i2c_master.o(i.drv_i2c_master_init)
    i.drv_i2c_master_read_dma                0x00016908   Section        0  drv_i2c_dma.o(i.drv_i2c_master_read_dma)
    i.drv_i2c_master_write_dma               0x00016984   Section        0  drv_i2c_dma.o(i.drv_i2c_master_write_dma)
    i.drv_i2c_master_write_read_cmd          0x000169c4   Section        0  drv_i2c_dma.o(i.drv_i2c_master_write_read_cmd)
    drv_i2c_master_write_read_cmd            0x000169c5   Thumb Code    46  drv_i2c_dma.o(i.drv_i2c_master_write_read_cmd)
    i.drv_i2c_s_enable_intr                  0x000169f4   Section        0  drv_i2c_slave.o(i.drv_i2c_s_enable_intr)
    i.drv_i2c_s_get_fifo_status              0x00016a28   Section        0  drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status)
    i.drv_i2c_s_set_callback                 0x00016a44   Section        0  drv_i2c_slave.o(i.drv_i2c_s_set_callback)
    i.drv_i2c_s_write_data                   0x00016a50   Section        0  drv_i2c_slave.o(i.drv_i2c_s_write_data)
    i.drv_i2c_set_dma_irq_callback           0x00016a70   Section        0  drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback)
    i.drv_i2c_slave_init                     0x00016ac0   Section        0  drv_i2c_slave.o(i.drv_i2c_slave_init)
    i.drv_i2c_slave_write_dma                0x00016b04   Section        0  drv_i2c_dma.o(i.drv_i2c_slave_write_dma)
    i.drv_lcdc_config_420_to_444_mode        0x00016b28   Section        0  drv_lcdc.o(i.drv_lcdc_config_420_to_444_mode)
    i.drv_lcdc_config_bypass                 0x00016b40   Section        0  drv_lcdc.o(i.drv_lcdc_config_bypass)
    i.drv_lcdc_config_cbcr                   0x00016b58   Section        0  drv_lcdc.o(i.drv_lcdc_config_cbcr)
    i.drv_lcdc_config_ccm                    0x00016b70   Section        0  drv_lcdc.o(i.drv_lcdc_config_ccm)
    i.drv_lcdc_config_disp_mode              0x00016ba0   Section        0  drv_lcdc.o(i.drv_lcdc_config_disp_mode)
    i.drv_lcdc_config_dpi_polarity           0x00016bb6   Section        0  drv_lcdc.o(i.drv_lcdc_config_dpi_polarity)
    i.drv_lcdc_config_dpi_timing             0x00016bda   Section        0  drv_lcdc.o(i.drv_lcdc_config_dpi_timing)
    i.drv_lcdc_config_endianness             0x00016c00   Section        0  drv_lcdc.o(i.drv_lcdc_config_endianness)
    i.drv_lcdc_config_horiz_flip             0x00016c16   Section        0  drv_lcdc.o(i.drv_lcdc_config_horiz_flip)
    i.drv_lcdc_config_input_size             0x00016c36   Section        0  drv_lcdc.o(i.drv_lcdc_config_input_size)
    i.drv_lcdc_config_int                    0x00016c42   Section        0  drv_lcdc.o(i.drv_lcdc_config_int)
    i.drv_lcdc_config_int_single             0x00016c60   Section        0  drv_lcdc.o(i.drv_lcdc_config_int_single)
    i.drv_lcdc_config_overwrite              0x00016c82   Section        0  drv_lcdc.o(i.drv_lcdc_config_overwrite)
    i.drv_lcdc_config_overwrite_rgb          0x00016ca4   Section        0  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    i.drv_lcdc_config_partial_display_area   0x00016cb0   Section        0  drv_lcdc.o(i.drv_lcdc_config_partial_display_area)
    i.drv_lcdc_config_partial_display_enable 0x00016cca   Section        0  drv_lcdc.o(i.drv_lcdc_config_partial_display_enable)
    i.drv_lcdc_config_src_parameter          0x00016cec   Section        0  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    i.drv_lcdc_config_thresh                 0x00016d5e   Section        0  drv_lcdc.o(i.drv_lcdc_config_thresh)
    i.drv_lcdc_config_upscaler               0x00016d66   Section        0  drv_lcdc.o(i.drv_lcdc_config_upscaler)
    i.drv_lcdc_config_yuv420_threshold       0x00016dc6   Section        0  drv_lcdc.o(i.drv_lcdc_config_yuv420_threshold)
    i.drv_lcdc_ctrl_flow                     0x00016dd0   Section        0  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    i.drv_lcdc_enable_shadow_reg             0x00016de2   Section        0  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    i.drv_lcdc_set_int                       0x00016e04   Section        0  drv_lcdc.o(i.drv_lcdc_set_int)
    i.drv_lcdc_start                         0x00016e38   Section        0  drv_lcdc.o(i.drv_lcdc_start)
    i.drv_lcdc_update_shadow_reg             0x00016e58   Section        0  drv_lcdc.o(i.drv_lcdc_update_shadow_reg)
    i.drv_memc_bypass_fifo_empty             0x00016e64   Section        0  drv_memc.o(i.drv_memc_bypass_fifo_empty)
    i.drv_memc_clear_status                  0x00016e74   Section        0  drv_memc.o(i.drv_memc_clear_status)
    i.drv_memc_enable_irq                    0x00016e80   Section        0  drv_memc.o(i.drv_memc_enable_irq)
    i.drv_memc_gen_a_tear_signal             0x00016ec0   Section        0  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    i.drv_memc_get_status                    0x00016ecc   Section        0  drv_memc.o(i.drv_memc_get_status)
    i.drv_memc_rate_transfer_sel             0x00016ede   Section        0  drv_memc.o(i.drv_memc_rate_transfer_sel)
    i.drv_memc_sel_vsync                     0x00016eee   Section        0  drv_memc.o(i.drv_memc_sel_vsync)
    i.drv_memc_set_data_mode                 0x00016efc   Section        0  drv_memc.o(i.drv_memc_set_data_mode)
    i.drv_memc_set_tear_hwclr                0x00016f08   Section        0  drv_memc.o(i.drv_memc_set_tear_hwclr)
    i.drv_memc_set_tear_mode                 0x00016f18   Section        0  drv_memc.o(i.drv_memc_set_tear_mode)
    i.drv_memc_set_tear_waveform             0x00016f28   Section        0  drv_memc.o(i.drv_memc_set_tear_waveform)
    i.drv_memc_set_yuv420_cfg                0x00016f4c   Section        0  drv_memc.o(i.drv_memc_set_yuv420_cfg)
    i.drv_param_get_picture_quality_setting  0x00016f5c   Section        0  drv_param_init.o(i.drv_param_get_picture_quality_setting)
    i.drv_param_init_get_ccm                 0x00016f6c   Section        0  drv_param_init.o(i.drv_param_init_get_ccm)
    i.drv_param_init_get_scld_filter_h       0x00016f74   Section        0  drv_param_init.o(i.drv_param_init_get_scld_filter_h)
    i.drv_param_init_get_scld_filter_v       0x00016f88   Section        0  drv_param_init.o(i.drv_param_init_get_scld_filter_v)
    i.drv_param_init_get_sclu_filter_h       0x00016f9c   Section        0  drv_param_init.o(i.drv_param_init_get_sclu_filter_h)
    i.drv_param_init_get_sclu_filter_v       0x00016fa4   Section        0  drv_param_init.o(i.drv_param_init_get_sclu_filter_v)
    i.drv_param_init_set_ccm                 0x00016fac   Section        0  drv_param_init.o(i.drv_param_init_set_ccm)
    i.drv_param_p2r_filter_init              0x00016fc0   Section        0  drv_param_init.o(i.drv_param_p2r_filter_init)
    i.drv_param_yuv420_filter_init           0x00016ffc   Section        0  drv_param_init.o(i.drv_param_yuv420_filter_init)
    i.drv_phy_get_pll_para                   0x00017030   Section        0  drv_phy_common.o(i.drv_phy_get_pll_para)
    i.drv_phy_get_rate_para                  0x00017090   Section        0  drv_phy_common.o(i.drv_phy_get_rate_para)
    i.drv_phy_test_clear                     0x000170e4   Section        0  drv_phy_common.o(i.drv_phy_test_clear)
    i.drv_phy_test_lock                      0x000170f4   Section        0  drv_phy_common.o(i.drv_phy_test_lock)
    i.drv_phy_test_write_1_byte              0x0001710c   Section        0  drv_phy_common.o(i.drv_phy_test_write_1_byte)
    i.drv_phy_test_write_2_byte              0x0001712c   Section        0  drv_phy_common.o(i.drv_phy_test_write_2_byte)
    i.drv_phy_test_write_code                0x00017152   Section        0  drv_phy_common.o(i.drv_phy_test_write_code)
    i.drv_phy_test_write_data                0x00017170   Section        0  drv_phy_common.o(i.drv_phy_test_write_data)
    drv_phy_test_write_data                  0x00017171   Thumb Code    32  drv_phy_common.o(i.drv_phy_test_write_data)
    i.drv_pwr_set_cp_mode                    0x00017190   Section        0  drv_pwr.o(i.drv_pwr_set_cp_mode)
    i.drv_pwr_set_pvd_mode                   0x000171b0   Section        0  drv_pwr.o(i.drv_pwr_set_pvd_mode)
    i.drv_pwr_set_system_clk_src             0x000171cc   Section        0  drv_pwr.o(i.drv_pwr_set_system_clk_src)
    i.drv_rx_phy_test_clear                  0x000171fc   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_clear)
    drv_rx_phy_test_clear                    0x000171fd   Thumb Code    12  drv_dsi_rx.o(i.drv_rx_phy_test_clear)
    i.drv_rx_phy_test_lock                   0x00017208   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_lock)
    drv_rx_phy_test_lock                     0x00017209   Thumb Code    16  drv_dsi_rx.o(i.drv_rx_phy_test_lock)
    i.drv_rx_phy_test_write_1_byte           0x00017218   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte)
    drv_rx_phy_test_write_1_byte             0x00017219   Thumb Code    20  drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte)
    i.drv_rx_phy_test_write_2_byte           0x0001722c   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte)
    drv_rx_phy_test_write_2_byte             0x0001722d   Thumb Code    22  drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte)
    i.drv_rxbr_clear_pkt_buffer              0x00017242   Section        0  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    i.drv_rxbr_clear_status                  0x00017248   Section        0  drv_rxbr.o(i.drv_rxbr_clear_status)
    i.drv_rxbr_enable_irq                    0x0001724c   Section        0  drv_rxbr.o(i.drv_rxbr_enable_irq)
    i.drv_rxbr_frame_drop_cfg                0x0001728c   Section        0  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    i.drv_rxbr_get_clk                       0x00017294   Section        0  drv_rxbr.o(i.drv_rxbr_get_clk)
    i.drv_rxbr_get_col_addr                  0x000172d0   Section        0  drv_rxbr.o(i.drv_rxbr_get_col_addr)
    i.drv_rxbr_get_cur_hline_rcv_cnt         0x000172d4   Section        0  drv_rxbr.o(i.drv_rxbr_get_cur_hline_rcv_cnt)
    i.drv_rxbr_get_hline_rcv_cfg             0x000172dc   Section        0  drv_rxbr.o(i.drv_rxbr_get_hline_rcv_cfg)
    i.drv_rxbr_get_int_source                0x000172ec   Section        0  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    drv_rxbr_get_int_source                  0x000172ed   Thumb Code    18  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    i.drv_rxbr_get_page_addr                 0x000172fe   Section        0  drv_rxbr.o(i.drv_rxbr_get_page_addr)
    i.drv_rxbr_get_status                    0x00017302   Section        0  hal_dsi_rx_ctrl.o(i.drv_rxbr_get_status)
    drv_rxbr_get_status                      0x00017303   Thumb Code    18  hal_dsi_rx_ctrl.o(i.drv_rxbr_get_status)
    i.drv_rxbr_get_status                    0x00017314   Section        0  hal_internal_vsync.o(i.drv_rxbr_get_status)
    drv_rxbr_get_status                      0x00017315   Thumb Code    18  hal_internal_vsync.o(i.drv_rxbr_get_status)
    i.drv_rxbr_hline_rcv0_cfg                0x00017326   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg)
    i.drv_rxbr_hline_rcv_cfg                 0x00017332   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    i.drv_rxbr_set_ack_pkt_header            0x0001733a   Section        0  drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header)
    i.drv_rxbr_set_cmd_filter                0x0001734e   Section        0  drv_rxbr.o(i.drv_rxbr_set_cmd_filter)
    i.drv_rxbr_set_color_format              0x0001741a   Section        0  drv_rxbr.o(i.drv_rxbr_set_color_format)
    i.drv_rxbr_set_inten                     0x0001742e   Section        0  drv_rxbr.o(i.drv_rxbr_set_inten)
    i.drv_rxbr_set_usr_cfg                   0x00017442   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    i.drv_rxbr_set_usr_col                   0x00017464   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    i.drv_rxbr_set_usr_row                   0x0001746c   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    i.drv_spi_m_read_data                    0x00017474   Section        0  drv_spi_master.o(i.drv_spi_m_read_data)
    i.drv_swire_set_int                      0x00017494   Section        0  drv_swire.o(i.drv_swire_set_int)
    i.drv_swire_set_power_down               0x000174dc   Section        0  drv_swire.o(i.drv_swire_set_power_down)
    i.drv_sys_cfg_clear_all_int              0x000174f8   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    i.drv_sys_cfg_clear_pending              0x00017504   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    i.drv_sys_cfg_sel_ap_rst_lvl_trig        0x0001752c   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig)
    i.drv_sys_cfg_sel_ap_rst_trig            0x00017544   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig)
    i.drv_sys_cfg_sel_gpio_group             0x00017560   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group)
    i.drv_sys_cfg_sel_int_trig               0x00017584   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig)
    i.drv_sys_cfg_set_dma_rx_req             0x000175a8   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req)
    i.drv_sys_cfg_set_dma_tx_req             0x000175b8   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req)
    i.drv_sys_cfg_set_int                    0x000175c8   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    i.drv_timer_clear_status_flags           0x000175ec   Section        0  drv_timer.o(i.drv_timer_clear_status_flags)
    drv_timer_clear_status_flags             0x000175ed   Thumb Code    26  drv_timer.o(i.drv_timer_clear_status_flags)
    i.drv_timer_enable                       0x00017606   Section        0  drv_timer.o(i.drv_timer_enable)
    i.drv_timer_get_instance                 0x00017628   Section        0  drv_timer.o(i.drv_timer_get_instance)
    i.drv_timer_get_prescaler                0x00017638   Section        0  drv_timer.o(i.drv_timer_get_prescaler)
    i.drv_timer_handle_interrupt             0x00017648   Section        0  drv_timer.o(i.drv_timer_handle_interrupt)
    drv_timer_handle_interrupt               0x00017649   Thumb Code    54  drv_timer.o(i.drv_timer_handle_interrupt)
    i.drv_timer_register_callback            0x00017684   Section        0  drv_timer.o(i.drv_timer_register_callback)
    i.drv_timer_set_compare_val              0x00017698   Section        0  drv_timer.o(i.drv_timer_set_compare_val)
    i.drv_timer_set_int                      0x000176a8   Section        0  drv_timer.o(i.drv_timer_set_int)
    i.drv_timer_set_prescaler                0x000176f0   Section        0  drv_timer.o(i.drv_timer_set_prescaler)
    i.drv_tx_phy_test_clear                  0x00017718   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_clear)
    drv_tx_phy_test_clear                    0x00017719   Thumb Code    10  drv_dsi_tx.o(i.drv_tx_phy_test_clear)
    i.drv_tx_phy_test_enter                  0x00017722   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    i.drv_tx_phy_test_exit                   0x0001773e   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    i.drv_tx_phy_test_write_1_byte           0x0001775a   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte)
    drv_tx_phy_test_write_1_byte             0x0001775b   Thumb Code    18  drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte)
    i.drv_tx_phy_test_write_2_byte           0x0001776c   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte)
    drv_tx_phy_test_write_2_byte             0x0001776d   Thumb Code    20  drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte)
    i.drv_tx_phy_test_write_code             0x00017780   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    drv_tx_phy_test_write_code               0x00017781   Thumb Code    16  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    i.drv_vidc_clear_irq                     0x00017790   Section        0  drv_vidc.o(i.drv_vidc_clear_irq)
    i.drv_vidc_enable                        0x00017798   Section        0  drv_vidc.o(i.drv_vidc_enable)
    i.drv_vidc_enable_irq                    0x000177b0   Section        0  drv_vidc.o(i.drv_vidc_enable_irq)
    i.drv_vidc_get_int_source                0x000177f0   Section        0  drv_vidc.o(i.drv_vidc_get_int_source)
    i.drv_vidc_module_enable                 0x00017818   Section        0  drv_vidc.o(i.drv_vidc_module_enable)
    i.drv_vidc_reset                         0x0001785c   Section        0  drv_vidc.o(i.drv_vidc_reset)
    i.drv_vidc_set_dst_parameter             0x00017862   Section        0  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    i.drv_vidc_set_enh_chr                   0x000178be   Section        0  drv_vidc.o(i.drv_vidc_set_enh_chr)
    i.drv_vidc_set_enh_chr2                  0x000178cc   Section        0  drv_vidc.o(i.drv_vidc_set_enh_chr2)
    i.drv_vidc_set_enh_lum                   0x000178de   Section        0  drv_vidc.o(i.drv_vidc_set_enh_lum)
    i.drv_vidc_set_gain                      0x000178ec   Section        0  drv_vidc.o(i.drv_vidc_set_gain)
    i.drv_vidc_set_irqen                     0x0001791c   Section        0  drv_vidc.o(i.drv_vidc_set_irqen)
    i.drv_vidc_set_p2r_hcoef0                0x00017930   Section        0  drv_vidc.o(i.drv_vidc_set_p2r_hcoef0)
    i.drv_vidc_set_p2r_hcoef1                0x00017938   Section        0  drv_vidc.o(i.drv_vidc_set_p2r_hcoef1)
    i.drv_vidc_set_p2r_hinitb                0x00017940   Section        0  drv_vidc.o(i.drv_vidc_set_p2r_hinitb)
    i.drv_vidc_set_p2r_hinitr                0x00017968   Section        0  drv_vidc.o(i.drv_vidc_set_p2r_hinitr)
    i.drv_vidc_set_p2r_step                  0x00017990   Section        0  drv_vidc.o(i.drv_vidc_set_p2r_step)
    i.drv_vidc_set_pu_ctrl                   0x00017998   Section        0  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    i.drv_vidc_set_pu_scld                   0x000179b8   Section        0  drv_vidc.o(i.drv_vidc_set_pu_scld)
    i.drv_vidc_set_scld_hcoef0               0x000179c6   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    i.drv_vidc_set_scld_hcoef1               0x000179d0   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    i.drv_vidc_set_scld_step                 0x000179da   Section        0  drv_vidc.o(i.drv_vidc_set_scld_step)
    i.drv_vidc_set_scld_vcoef0               0x000179ec   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    i.drv_vidc_set_scld_vcoef1               0x000179f6   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    i.drv_vidc_set_sclu_hcoef0c              0x00017a00   Section        0  drv_vidc.o(i.drv_vidc_set_sclu_hcoef0c)
    i.drv_vidc_set_sclu_hcoef0y              0x00017a0a   Section        0  drv_vidc.o(i.drv_vidc_set_sclu_hcoef0y)
    i.drv_vidc_set_sclu_hcoef1c              0x00017a14   Section        0  drv_vidc.o(i.drv_vidc_set_sclu_hcoef1c)
    i.drv_vidc_set_sclu_hcoef1y              0x00017a1e   Section        0  drv_vidc.o(i.drv_vidc_set_sclu_hcoef1y)
    i.drv_vidc_set_sclu_vcoef0c              0x00017a28   Section        0  drv_vidc.o(i.drv_vidc_set_sclu_vcoef0c)
    i.drv_vidc_set_sclu_vcoef0y              0x00017a32   Section        0  drv_vidc.o(i.drv_vidc_set_sclu_vcoef0y)
    i.drv_vidc_set_sclu_vcoef1c              0x00017a3c   Section        0  drv_vidc.o(i.drv_vidc_set_sclu_vcoef1c)
    i.drv_vidc_set_sclu_vcoef1y              0x00017a46   Section        0  drv_vidc.o(i.drv_vidc_set_sclu_vcoef1y)
    i.drv_vidc_set_src_parameter             0x00017a50   Section        0  drv_vidc.o(i.drv_vidc_set_src_parameter)
    i.drv_vidc_set_y4t2_hcoef0               0x00017a74   Section        0  drv_vidc.o(i.drv_vidc_set_y4t2_hcoef0)
    i.drv_vidc_set_y4t2_hcoef1               0x00017a7e   Section        0  drv_vidc.o(i.drv_vidc_set_y4t2_hcoef1)
    i.drv_vidc_set_y4t2_vcoef0               0x00017a88   Section        0  drv_vidc.o(i.drv_vidc_set_y4t2_vcoef0)
    i.drv_vidc_set_y4t2_vcoef1               0x00017a92   Section        0  drv_vidc.o(i.drv_vidc_set_y4t2_vcoef1)
    i.drv_wdg_clear_counter                  0x00017a9c   Section        0  drv_wdg.o(i.drv_wdg_clear_counter)
    i.drv_wdg_clear_edge_flag                0x00017aac   Section        0  drv_wdg.o(i.drv_wdg_clear_edge_flag)
    drv_wdg_clear_edge_flag                  0x00017aad   Thumb Code    12  drv_wdg.o(i.drv_wdg_clear_edge_flag)
    i.drv_wdg_read_edge_flag                 0x00017abc   Section        0  drv_wdg.o(i.drv_wdg_read_edge_flag)
    drv_wdg_read_edge_flag                   0x00017abd   Thumb Code    10  drv_wdg.o(i.drv_wdg_read_edge_flag)
    i.drv_wdg_set_int                        0x00017acc   Section        0  drv_wdg.o(i.drv_wdg_set_int)
    i.fls_clear_irq_status                   0x00017b00   Section        0  drv_fls.o(i.fls_clear_irq_status)
    i.fputc                                  0x00017b06   Section        0  tau_log.o(i.fputc)
    i.hal_dsi_rx_ctrl_create_handle          0x00017b1c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    i.hal_dsi_rx_ctrl_deinit                 0x00017b4c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit)
    i.hal_dsi_rx_ctrl_dsc_async_handler      0x00017be8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler)
    i.hal_dsi_rx_ctrl_gen_a_tear_signal      0x00017c6c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal)
    i.hal_dsi_rx_ctrl_get_max_ret_size       0x00017c94   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size)
    i.hal_dsi_rx_ctrl_init                   0x00017cbc   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    i.hal_dsi_rx_ctrl_init_clk               0x00017d20   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    hal_dsi_rx_ctrl_init_clk                 0x00017d21   Thumb Code   218  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    i.hal_dsi_rx_ctrl_init_dsc_dec           0x00017e44   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsc_dec)
    hal_dsi_rx_ctrl_init_dsc_dec             0x00017e45   Thumb Code    66  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsc_dec)
    i.hal_dsi_rx_ctrl_init_dsi_rx            0x00017e8c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    hal_dsi_rx_ctrl_init_dsi_rx              0x00017e8d   Thumb Code   172  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    i.hal_dsi_rx_ctrl_init_memc              0x00017f58   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    hal_dsi_rx_ctrl_init_memc                0x00017f59   Thumb Code   186  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    i.hal_dsi_rx_ctrl_init_rxbr              0x0001801c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    hal_dsi_rx_ctrl_init_rxbr                0x0001801d   Thumb Code   314  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    i.hal_dsi_rx_ctrl_init_vidc              0x00018168   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    hal_dsi_rx_ctrl_init_vidc                0x00018169   Thumb Code   892  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    i.hal_dsi_rx_ctrl_pre_init_pps           0x000184f0   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    i.hal_dsi_rx_ctrl_send_ack_cmd           0x0001852c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd)
    i.hal_dsi_rx_ctrl_set_cus_sync_line      0x0001861c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line)
    i.hal_dsi_rx_ctrl_set_hw_tear_mode       0x00018650   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode)
    i.hal_dsi_rx_ctrl_set_ipi_cfg            0x00018684   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    hal_dsi_rx_ctrl_set_ipi_cfg              0x00018685   Thumb Code    48  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    i.hal_dsi_rx_ctrl_set_rxbr_clk           0x000186b8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk)
    hal_dsi_rx_ctrl_set_rxbr_clk             0x000186b9   Thumb Code   114  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk)
    i.hal_dsi_rx_ctrl_set_sw_tear_mode       0x0001872c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode)
    i.hal_dsi_rx_ctrl_start                  0x00018760   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    i.hal_dsi_rx_ctrl_stop                   0x0001879c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop)
    i.hal_dsi_rx_ctrl_toggle_resolution      0x000187e4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    i.hal_dsi_tx_calc_video_chunks           0x00018804   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks)
    hal_dsi_tx_calc_video_chunks             0x00018805   Thumb Code   384  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks)
    i.hal_dsi_tx_config_params_for_lane_rate 0x00018994   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate)
    hal_dsi_tx_config_params_for_lane_rate   0x00018995   Thumb Code    42  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate)
    i.hal_dsi_tx_count_lane_rate             0x000189c8   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate)
    hal_dsi_tx_count_lane_rate               0x000189c9   Thumb Code   950  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate)
    i.hal_dsi_tx_ctrl_create_handle          0x00018d88   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    i.hal_dsi_tx_ctrl_deinit                 0x00018db4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit)
    i.hal_dsi_tx_ctrl_enter_init_panel_mode  0x00018dfc   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode)
    i.hal_dsi_tx_ctrl_exit_init_panel_mode   0x00018e48   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode)
    i.hal_dsi_tx_ctrl_init                   0x00018e6c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    i.hal_dsi_tx_ctrl_init_clk               0x00018f30   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    hal_dsi_tx_ctrl_init_clk                 0x00018f31   Thumb Code    36  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    i.hal_dsi_tx_ctrl_panel_reset_pin        0x00018f54   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin)
    i.hal_dsi_tx_ctrl_set_ccm                0x00018f60   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm)
    i.hal_dsi_tx_ctrl_set_overwrite_rgb      0x00018f80   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    i.hal_dsi_tx_ctrl_set_partial_disp       0x00018f94   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp)
    i.hal_dsi_tx_ctrl_set_partial_disp_area  0x00018fa4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area)
    i.hal_dsi_tx_ctrl_start                  0x00018fc8   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    i.hal_dsi_tx_ctrl_stop                   0x00019028   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop)
    i.hal_dsi_tx_ctrl_write_array_cmd        0x0001906c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd)
    i.hal_dsi_tx_ctrl_write_cmd              0x00019208   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    i.hal_dsi_tx_init_data_mode              0x00019358   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode)
    hal_dsi_tx_init_data_mode                0x00019359   Thumb Code    36  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode)
    i.hal_dsi_tx_init_dpi_cfg                0x00019380   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg)
    hal_dsi_tx_init_dpi_cfg                  0x00019381   Thumb Code    42  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg)
    i.hal_dsi_tx_init_interrupt              0x000193b0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt)
    hal_dsi_tx_init_interrupt                0x000193b1   Thumb Code    28  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt)
    i.hal_dsi_tx_init_phy_cfg                0x000193d0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    hal_dsi_tx_init_phy_cfg                  0x000193d1   Thumb Code    28  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    i.hal_dsi_tx_init_remains                0x000193f0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains)
    hal_dsi_tx_init_remains                  0x000193f1   Thumb Code   142  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains)
    i.hal_dsi_tx_init_video_mode             0x00019484   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode)
    hal_dsi_tx_init_video_mode               0x00019485   Thumb Code    82  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode)
    i.hal_dsi_tx_send_cmd                    0x000194dc   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    hal_dsi_tx_send_cmd                      0x000194dd   Thumb Code    60  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    i.hal_gpio_ctrl_eint                     0x00019520   Section        0  hal_gpio.o(i.hal_gpio_ctrl_eint)
    i.hal_gpio_get_input_data                0x00019538   Section        0  hal_gpio.o(i.hal_gpio_get_input_data)
    i.hal_gpio_init_eint                     0x0001954c   Section        0  hal_gpio.o(i.hal_gpio_init_eint)
    i.hal_gpio_init_input                    0x0001958c   Section        0  hal_gpio.o(i.hal_gpio_init_input)
    i.hal_gpio_init_output                   0x000195ac   Section        0  hal_gpio.o(i.hal_gpio_init_output)
    i.hal_gpio_reg_eint_cb                   0x000195d4   Section        0  hal_gpio.o(i.hal_gpio_reg_eint_cb)
    i.hal_gpio_set_ap_reset_int              0x000195ec   Section        0  hal_gpio.o(i.hal_gpio_set_ap_reset_int)
    i.hal_gpio_set_mode                      0x0001963c   Section        0  hal_gpio.o(i.hal_gpio_set_mode)
    i.hal_gpio_set_output_data               0x0001969c   Section        0  hal_gpio.o(i.hal_gpio_set_output_data)
    i.hal_gpio_set_pull_state                0x000196a4   Section        0  hal_gpio.o(i.hal_gpio_set_pull_state)
    i.hal_i2c_m_dma_init                     0x000196c4   Section        0  hal_i2c_master.o(i.hal_i2c_m_dma_init)
    i.hal_i2c_m_dma_read                     0x00019730   Section        0  hal_i2c_master.o(i.hal_i2c_m_dma_read)
    i.hal_i2c_m_dma_write                    0x0001975c   Section        0  hal_i2c_master.o(i.hal_i2c_m_dma_write)
    i.hal_i2c_m_transfer_complate            0x00019784   Section        0  hal_i2c_master.o(i.hal_i2c_m_transfer_complate)
    i.hal_i2c_master_irq_callback            0x000197a4   Section        0  hal_i2c_master.o(i.hal_i2c_master_irq_callback)
    hal_i2c_master_irq_callback              0x000197a5   Thumb Code    24  hal_i2c_master.o(i.hal_i2c_master_irq_callback)
    i.hal_i2c_s_dma_user_callback            0x000197c4   Section        0  hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback)
    hal_i2c_s_dma_user_callback              0x000197c5   Thumb Code    12  hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback)
    i.hal_i2c_s_dma_write                    0x000197d4   Section        0  hal_i2c_slave.o(i.hal_i2c_s_dma_write)
    i.hal_i2c_s_init                         0x00019810   Section        0  hal_i2c_slave.o(i.hal_i2c_s_init)
    i.hal_i2c_s_nonblocking_read             0x0001987c   Section        0  hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read)
    i.hal_i2c_s_set_transfer                 0x00019890   Section        0  hal_i2c_slave.o(i.hal_i2c_s_set_transfer)
    i.hal_i2c_slave_irq_callback             0x0001989c   Section        0  hal_i2c_slave.o(i.hal_i2c_slave_irq_callback)
    hal_i2c_slave_irq_callback               0x0001989d   Thumb Code   306  hal_i2c_slave.o(i.hal_i2c_slave_irq_callback)
    i.hal_internal_init_memc                 0x000199ec   Section        0  hal_internal_vsync.o(i.hal_internal_init_memc)
    i.hal_internal_sync_get_fb_setting       0x00019a9c   Section        0  hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting)
    i.hal_internal_sync_input_resolution_change 0x00019aac   Section        0  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    i.hal_internal_sync_set_fb_setting_manual 0x00019cf8   Section        0  hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual)
    i.hal_internal_vsync_deinit              0x00019e80   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    i.hal_internal_vsync_get_rx_state        0x00019e9c   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state)
    i.hal_internal_vsync_get_sync_line       0x00019ea8   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    i.hal_internal_vsync_get_tx_state        0x00019ec4   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    i.hal_internal_vsync_get_y2t4_use_sclu   0x00019ed0   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_y2t4_use_sclu)
    i.hal_internal_vsync_init_rx             0x00019ef0   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    i.hal_internal_vsync_init_tx             0x00019fac   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    i.hal_internal_vsync_set_auto_hw_filter  0x0001a050   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter)
    i.hal_internal_vsync_set_rx_state        0x0001a16c   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    i.hal_internal_vsync_set_sync_line       0x0001a184   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line)
    i.hal_internal_vsync_set_tear_mode       0x0001a1a4   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    i.hal_internal_vsync_set_tx_state        0x0001a1ec   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    i.hal_lcdc_config_ccm                    0x0001a230   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm)
    hal_lcdc_config_ccm                      0x0001a231   Thumb Code    30  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm)
    i.hal_lcdc_config_remains                0x0001a254   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains)
    hal_lcdc_config_remains                  0x0001a255   Thumb Code    80  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains)
    i.hal_lcdc_config_rgb_to_pentile         0x0001a2a8   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile)
    hal_lcdc_config_rgb_to_pentile           0x0001a2a9   Thumb Code    14  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile)
    i.hal_lcdc_config_upscaler               0x0001a2bc   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler)
    hal_lcdc_config_upscaler                 0x0001a2bd   Thumb Code   444  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler)
    i.hal_lcdc_config_yuv_to_rgb             0x0001a484   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_yuv_to_rgb)
    hal_lcdc_config_yuv_to_rgb               0x0001a485   Thumb Code    26  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_yuv_to_rgb)
    i.hal_lcdc_init_cfg                      0x0001a4a4   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    hal_lcdc_init_cfg                        0x0001a4a5   Thumb Code    58  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    i.hal_lcdc_init_clk                      0x0001a4e0   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    hal_lcdc_init_clk                        0x0001a4e1   Thumb Code   376  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    i.hal_lcdc_init_interrupt                0x0001a660   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt)
    hal_lcdc_init_interrupt                  0x0001a661   Thumb Code    58  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt)
    i.hal_spi_m_clear_rxfifo                 0x0001a6a0   Section        0  hal_spi_master.o(i.hal_spi_m_clear_rxfifo)
    i.hal_swire_open                         0x0001a6ae   Section        0  hal_swire.o(i.hal_swire_open)
    i.hal_system_enable_systick              0x0001a6c4   Section        0  hal_system.o(i.hal_system_enable_systick)
    i.hal_system_init                        0x0001a6cc   Section        0  hal_system.o(i.hal_system_init)
    i.hal_system_init_console                0x0001a754   Section        0  hal_system.o(i.hal_system_init_console)
    i.hal_system_set_pvd                     0x0001a770   Section        0  hal_system.o(i.hal_system_set_pvd)
    i.hal_system_set_vcc                     0x0001a778   Section        0  hal_system.o(i.hal_system_set_vcc)
    i.hal_timer_init                         0x0001a780   Section        0  hal_timer.o(i.hal_timer_init)
    i.hal_timer_start                        0x0001a79c   Section        0  hal_timer.o(i.hal_timer_start)
    i.hal_timer_stop                         0x0001a7e4   Section        0  hal_timer.o(i.hal_timer_stop)
    i.hal_uart_init                          0x0001a80c   Section        0  hal_uart.o(i.hal_uart_init)
    i.hal_uart_transmit_blocking             0x0001a898   Section        0  hal_uart.o(i.hal_uart_transmit_blocking)
    i.handle_init                            0x0001a8a8   Section        0  irq_redirect .o(i.handle_init)
    i.init_mipi_tx                           0x0001a9b0   Section        0  ap_demo.o(i.init_mipi_tx)
    init_mipi_tx                             0x0001a9b1   Thumb Code   100  ap_demo.o(i.init_mipi_tx)
    i.init_panel                             0x0001aa18   Section        0  ap_demo.o(i.init_panel)
    init_panel                               0x0001aa19   Thumb Code   134  ap_demo.o(i.init_panel)
    i.main                                   0x0001aad0   Section        0  main.o(i.main)
    i.open_mipi_rx                           0x0001aadc   Section        0  ap_demo.o(i.open_mipi_rx)
    open_mipi_rx                             0x0001aadd   Thumb Code   140  ap_demo.o(i.open_mipi_rx)
    i.pps_update_handle                      0x0001ab80   Section        0  ap_demo.o(i.pps_update_handle)
    pps_update_handle                        0x0001ab81   Thumb Code    78  ap_demo.o(i.pps_update_handle)
    i.rx_get_dcs_packet_data                 0x0001abd4   Section        0  hal_internal_vsync.o(i.rx_get_dcs_packet_data)
    rx_get_dcs_packet_data                   0x0001abd5   Thumb Code   740  hal_internal_vsync.o(i.rx_get_dcs_packet_data)
    i.rx_partial_update                      0x0001afe4   Section        0  hal_internal_vsync.o(i.rx_partial_update)
    rx_partial_update                        0x0001afe5   Thumb Code   302  hal_internal_vsync.o(i.rx_partial_update)
    i.rx_receive_packet                      0x0001b120   Section        0  hal_internal_vsync.o(i.rx_receive_packet)
    rx_receive_packet                        0x0001b121   Thumb Code    90  hal_internal_vsync.o(i.rx_receive_packet)
    i.rx_receive_pps                         0x0001b184   Section        0  hal_internal_vsync.o(i.rx_receive_pps)
    rx_receive_pps                           0x0001b185   Thumb Code   266  hal_internal_vsync.o(i.rx_receive_pps)
    i.send_panel_init_code                   0x0001b304   Section        0  ap_demo.o(i.send_panel_init_code)
    send_panel_init_code                     0x0001b305   Thumb Code    42  ap_demo.o(i.send_panel_init_code)
    i.soft_disable_mipi_timer_init           0x0001b330   Section        0  ap_demo.o(i.soft_disable_mipi_timer_init)
    soft_disable_mipi_timer_init             0x0001b331   Thumb Code    32  ap_demo.o(i.soft_disable_mipi_timer_init)
    i.soft_gen_te                            0x0001b390   Section        0  hal_internal_vsync.o(i.soft_gen_te)
    soft_gen_te                              0x0001b391   Thumb Code   116  hal_internal_vsync.o(i.soft_gen_te)
    i.soft_timer3_cb                         0x0001b41c   Section        0  ap_demo.o(i.soft_timer3_cb)
    soft_timer3_cb                           0x0001b41d   Thumb Code    36  ap_demo.o(i.soft_timer3_cb)
    i.tp_heartbeat_exec                      0x0001b44c   Section        0  ap_demo.o(i.tp_heartbeat_exec)
    i.tx_display_on                          0x0001b494   Section        0  ap_demo.o(i.tx_display_on)
    tx_display_on                            0x0001b495   Thumb Code    16  ap_demo.o(i.tx_display_on)
    i.tx_panel_reset                         0x0001b4a8   Section        0  ap_demo.o(i.tx_panel_reset)
    tx_panel_reset                           0x0001b4a9   Thumb Code    40  ap_demo.o(i.tx_panel_reset)
    i.vpre_err_reset                         0x0001b4d0   Section        0  hal_internal_vsync.o(i.vpre_err_reset)
    vpre_err_reset                           0x0001b4d1   Thumb Code   184  hal_internal_vsync.o(i.vpre_err_reset)
    i.vsync_set_te_mode                      0x0001b5a0   Section        0  hal_internal_vsync.o(i.vsync_set_te_mode)
    vsync_set_te_mode                        0x0001b5a1   Thumb Code   254  hal_internal_vsync.o(i.vsync_set_te_mode)
    .constdata                               0x0001b73c   Section      236  ap_demo.o(.constdata)
    g_cus_rx_dcs_execute_table               0x0001b73c   Data         108  ap_demo.o(.constdata)
    .constdata                               0x0001b828   Section     8528  app_tp_for_custom_s8.o(.constdata)
    .constdata                               0x0001d978   Section      210  hal_gpio.o(.constdata)
    s_gpio_map                               0x0001d978   Data         120  hal_gpio.o(.constdata)
    s_gpio_perf                              0x0001d9f0   Data          90  hal_gpio.o(.constdata)
    .constdata                               0x0001da4c   Section      272  drv_param_init.o(.constdata)
    .constdata                               0x0001db5c   Section      390  drv_phy_common.o(.constdata)
    phy_para_mapping_h                       0x0001db5c   Data         184  drv_phy_common.o(.constdata)
    phy_para_mapping_l                       0x0001dc14   Data         128  drv_phy_common.o(.constdata)
    phy_data_high_map                        0x0001dc94   Data          48  drv_phy_common.o(.constdata)
    phy_data_lp_map                          0x0001dcc4   Data          30  drv_phy_common.o(.constdata)
    .conststring                             0x0001dce4   Section       72  hal_dsi_rx_ctrl.o(.conststring)
    .conststring                             0x0001dd2c   Section      296  hal_internal_vsync.o(.conststring)
    .ARM.__AT_0x00070100                     0x00070100   Section      192  irq_redirect .o(.ARM.__AT_0x00070100)
    .data                                    0x000701d0   Section    10009  ap_demo.o(.data)
    start_display_on                         0x000701d0   Data           1  ap_demo.o(.data)
    g_need_enter_sleep_mode                  0x000701d1   Data           1  ap_demo.o(.data)
    g_mipi_path_off                          0x000701d2   Data           1  ap_demo.o(.data)
    phone_off_flag                           0x000701d3   Data           1  ap_demo.o(.data)
    g_exit_sleep_mode                        0x000701d4   Data           1  ap_demo.o(.data)
    panel_display_done                       0x000701d5   Data           1  ap_demo.o(.data)
    g_calibration_flag                       0x000701da   Data           1  ap_demo.o(.data)
    b3_read_flag                             0x000701db   Data           1  ap_demo.o(.data)
    c8_read_flag                             0x000701dc   Data           1  ap_demo.o(.data)
    c9_read_flag                             0x000701dd   Data           1  ap_demo.o(.data)
    bl_adj_flag                              0x000701e0   Data           1  ap_demo.o(.data)
    flag_5a                                  0x000701e2   Data           1  ap_demo.o(.data)
    g_rx_ctrl_handle                         0x000701f4   Data           4  ap_demo.o(.data)
    g_tx_ctrl_handle                         0x000701f8   Data           4  ap_demo.o(.data)
    value_reg_df                             0x00070204   Data           4  ap_demo.o(.data)
    .data                                    0x000728ea   Section      228  app_tp_for_custom_s8.o(.data)
    app_tp_count                             0x000728f4   Data           1  app_tp_for_custom_s8.o(.data)
    phone_85_flag                            0x000728f5   Data           1  app_tp_for_custom_s8.o(.data)
    phone_F6_flag                            0x000728f6   Data           1  app_tp_for_custom_s8.o(.data)
    phone_E4_flag                            0x000728f7   Data           1  app_tp_for_custom_s8.o(.data)
    phone_72_flag                            0x000728f8   Data           1  app_tp_for_custom_s8.o(.data)
    phone_75_flag                            0x000728f9   Data           1  app_tp_for_custom_s8.o(.data)
    phone_92_flag                            0x000728fa   Data           1  app_tp_for_custom_s8.o(.data)
    phone_74_flag                            0x000728fb   Data           1  app_tp_for_custom_s8.o(.data)
    u16CoordY                                0x000728fe   Data           2  app_tp_for_custom_s8.o(.data)
    u16CoordX                                0x00072900   Data           2  app_tp_for_custom_s8.o(.data)
    u16CoordY_back                           0x00072902   Data           2  app_tp_for_custom_s8.o(.data)
    u16CoordX_back                           0x00072904   Data           2  app_tp_for_custom_s8.o(.data)
    .data                                    0x000729ce   Section        1  app_tp_for_custom_s8.o(.data)
    .data                                    0x000729cf   Section        1  app_tp_for_custom_s8.o(.data)
    .data                                    0x000729d0   Section        1  app_tp_for_custom_s8.o(.data)
    .data                                    0x000729d1   Section        3  app_tp_for_custom_s8.o(.data)
    .data                                    0x000729d4   Section        5  app_tp_for_custom_s8.o(.data)
    .data                                    0x000729dc   Section       48  app_tp_for_custom_s8.o(.data)
    .data                                    0x00072a0c   Section       49  app_tp_transfer.o(.data)
    s_spim_write                             0x00072a0c   Data           1  app_tp_transfer.o(.data)
    s_screen_int_flag                        0x00072a0d   Data           1  app_tp_transfer.o(.data)
    s_phone_reset_flag                       0x00072a0e   Data           1  app_tp_transfer.o(.data)
    s_screen_int_transfer_status             0x00072a0f   Data           1  app_tp_transfer.o(.data)
    s_screen_const_transfer_count            0x00072a11   Data           1  app_tp_transfer.o(.data)
    screen_int_transfer_count                0x00072a12   Data           1  app_tp_transfer.o(.data)
    screen_int_transfer_buffer_ready         0x00072a13   Data           1  app_tp_transfer.o(.data)
    .data                                    0x00072a40   Section        8  hal_dsi_rx_ctrl.o(.data)
    g_hw_auto_filter                         0x00072a40   Data           1  hal_dsi_rx_ctrl.o(.data)
    g_esc_clk                                0x00072a44   Data           4  hal_dsi_rx_ctrl.o(.data)
    .data                                    0x00072a48   Section        1  hal_i2c_master.o(.data)
    s_i2c_m_transfer_end                     0x00072a48   Data           1  hal_i2c_master.o(.data)
    .data                                    0x00072a4c   Section       28  hal_i2c_slave.o(.data)
    s_txbuffer_complate                      0x00072a4c   Data           1  hal_i2c_slave.o(.data)
    s_i2c_s_dma_end                          0x00072a4d   Data           1  hal_i2c_slave.o(.data)
    s_i2c_s_receive_cnt                      0x00072a4e   Data           1  hal_i2c_slave.o(.data)
    s_hal_slave_rxbuffer                     0x00072a50   Data           4  hal_i2c_slave.o(.data)
    s_hal_slave_rxbuffer_size                0x00072a54   Data           4  hal_i2c_slave.o(.data)
    hal_i2c_s_callback                       0x00072a58   Data           4  hal_i2c_slave.o(.data)
    s_receive_count                          0x00072a5c   Data           4  hal_i2c_slave.o(.data)
    s_tx_buffer_t                            0x00072a60   Data           4  hal_i2c_slave.o(.data)
    tx_sum                                   0x00072a64   Data           4  hal_i2c_slave.o(.data)
    .data                                    0x00072a68   Section       18  norflash.o(.data)
    tmprg                                    0x00072a70   Data           4  norflash.o(.data)
    .data                                    0x00072a7c   Section       12  drv_common.o(.data)
    s_my_tick                                0x00072a7c   Data           4  drv_common.o(.data)
    .data                                    0x00072a88   Section        4  drv_gpio.o(.data)
    g_ap_reset_cb                            0x00072a88   Data           4  drv_gpio.o(.data)
    .data                                    0x00072a8c   Section        8  drv_i2c_dma.o(.data)
    i2c0_dma_callback                        0x00072a8c   Data           4  drv_i2c_dma.o(.data)
    i2c1_dma_callback                        0x00072a90   Data           4  drv_i2c_dma.o(.data)
    .data                                    0x00072a94   Section        4  drv_i2c_master.o(.data)
    i2c1_intr_callback                       0x00072a94   Data           4  drv_i2c_master.o(.data)
    .data                                    0x00072a98   Section        8  drv_i2c_slave.o(.data)
    i2c0_intr_callback                       0x00072a98   Data           4  drv_i2c_slave.o(.data)
    .data                                    0x00072aa0   Section     1612  drv_param_init.o(.data)
    .data                                    0x000730ec   Section        4  drv_spi_master.o(.data)
    SPIM_intr_callback                       0x000730ec   Data           4  drv_spi_master.o(.data)
    .data                                    0x000730f0   Section        8  drv_swire.o(.data)
    s_swire_cb                               0x000730f0   Data           8  drv_swire.o(.data)
    .data                                    0x000730f8   Section        1  drv_sys_cfg.o(.data)
    sg_ap_rstn_trigger_type                  0x000730f8   Data           1  drv_sys_cfg.o(.data)
    .data                                    0x000730fc   Section       80  drv_timer.o(.data)
    sg_timer_info                            0x000730fc   Data          80  drv_timer.o(.data)
    .data                                    0x0007314c   Section        4  hal_internal_vsync.o(.data)
    sg_cur_te_info                           0x0007314c   Data           4  hal_internal_vsync.o(.data)
    .data                                    0x00073150   Section        8  drv_chip_info.o(.data)
    sg_chip_ver                              0x00073150   Data           1  drv_chip_info.o(.data)
    sg_3k_flag                               0x00073154   Data           4  drv_chip_info.o(.data)
    .data                                    0x00073158   Section       12  drv_pwm.o(.data)
    s_pwm_type                               0x00073158   Data           1  drv_pwm.o(.data)
    s_pwm_cb                                 0x0007315c   Data           8  drv_pwm.o(.data)
    .data                                    0x00073164   Section        8  drv_uart.o(.data)
    s_UartFcrReg                             0x00073164   Data           4  drv_uart.o(.data)
    uart_userData                            0x00073168   Data           4  drv_uart.o(.data)
    .data                                    0x0007316c   Section       12  drv_wdg.o(.data)
    sg_wdg_repeat                            0x0007316c   Data           1  drv_wdg.o(.data)
    sg_wdg_cb                                0x00073170   Data           8  drv_wdg.o(.data)
    .data                                    0x00073178   Section        4  stdout.o(.data)
    .bss                                     0x0007317c   Section      412  app_tp_transfer.o(.bss)
    s_screen_read_buffer                     0x0007317c   Data         200  app_tp_transfer.o(.bss)
    s_phone_read_buffer                      0x00073244   Data         200  app_tp_transfer.o(.bss)
    .bss                                     0x00073318   Section      184  hal_dsi_rx_ctrl.o(.bss)
    g_rx_ctrl_handle                         0x00073318   Data         184  hal_dsi_rx_ctrl.o(.bss)
    .bss                                     0x000733d0   Section       64  hal_dsi_tx_ctrl.o(.bss)
    g_tx_ctrl_handle                         0x000733d0   Data          64  hal_dsi_tx_ctrl.o(.bss)
    .bss                                     0x00073410   Section      256  tau_log.o(.bss)
    .bss                                     0x00073510   Section       60  hal_uart.o(.bss)
    .bss                                     0x0007354c   Section       24  drv_dma.o(.bss)
    s_dma_handle                             0x0007354c   Data          24  drv_dma.o(.bss)
    .bss                                     0x00073564   Section       64  drv_gpio.o(.bss)
    s_gpio_cb                                0x00073564   Data          64  drv_gpio.o(.bss)
    .bss                                     0x000735a4   Section       24  drv_i2c_dma.o(.bss)
    i2c0_dma_slave_handle                    0x000735a4   Data          12  drv_i2c_dma.o(.bss)
    i2c1_dma_master_handle                   0x000735b0   Data          12  drv_i2c_dma.o(.bss)
    .bss                                     0x000735bc   Section     2764  dcs_packet_fifo.o(.bss)
    .bss                                     0x00074088   Section     2408  hal_internal_vsync.o(.bss)
    g_vsync_hande                            0x00074088   Data          72  hal_internal_vsync.o(.bss)
    g_dcs_execute_table                      0x000740d0   Data        2048  hal_internal_vsync.o(.bss)
    g_imm_buffer                             0x000748d0   Data         255  hal_internal_vsync.o(.bss)
    sg_te_info                               0x000749d0   Data          12  hal_internal_vsync.o(.bss)
    g_imm_packet                             0x000749dc   Data          20  hal_internal_vsync.o(.bss)
    .bss                                     0x000749f0   Section       32  hal_spi_slave.o(.bss)
    STACK                                    0x00074a10   Section     4096  startup_armcm0.o(STACK)

    Global Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    BuildAttributes$$THM_ISAv3M$S$PE$A:L22$X:L11$S22$IEEE1$IW$USESV6$~STKCKD$USESV7$~SHL$OTIME$ROPI$IEEEJ$EBA8$MICROLIB$REQ8$PRES8$EABIv2 0x00000000   Number         0  anon$$obj.o ABSOLUTE
    __ARM_use_no_argv                        0x00000000   Number         0  main.o ABSOLUTE
    _printf_a                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_c                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_charcount                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_d                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_e                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_f                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_flags                            0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_dec                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_hex                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_g                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_i                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_int_dec                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_l                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ll                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lld                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lli                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llo                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llu                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llx                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_dec                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_hex                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_oct                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ls                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_mbtowc                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_n                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_o                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_p                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_percent                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_pre_padding                      0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_return_value                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_s                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_sizespec                         0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_str                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_signed                  0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_unsigned                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_u                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wctomb                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_widthprec                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_x                                0x00000000   Number         0  stubs.o ABSOLUTE
    __cpp_initialize__aeabi_                  - Undefined Weak Reference
    __cxa_finalize                            - Undefined Weak Reference
    _clock_init                               - Undefined Weak Reference
    _microlib_exit                            - Undefined Weak Reference
    __Vectors_Size                           0x000000c0   Number         0  startup_armcm0.o ABSOLUTE
    __Vectors                                0x00010000   Data           4  startup_armcm0.o(RESET)
    __Vectors_End                            0x000100c0   Data           0  startup_armcm0.o(RESET)
    __main                                   0x000100c1   Thumb Code     0  entry.o(.ARM.Collect$$$$00000000)
    _main_stk                                0x000100c1   Thumb Code     0  entry2.o(.ARM.Collect$$$$00000001)
    _main_scatterload                        0x000100c5   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    __main_after_scatterload                 0x000100c9   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    _main_clock                              0x000100c9   Thumb Code     0  entry7b.o(.ARM.Collect$$$$00000008)
    _main_cpp_init                           0x000100c9   Thumb Code     0  entry8b.o(.ARM.Collect$$$$0000000A)
    _main_init                               0x000100c9   Thumb Code     0  entry9a.o(.ARM.Collect$$$$0000000B)
    __rt_final_cpp                           0x000100d1   Thumb Code     0  entry10a.o(.ARM.Collect$$$$0000000D)
    __rt_final_exit                          0x000100d1   Thumb Code     0  entry11a.o(.ARM.Collect$$$$0000000F)
    Reset_Handler                            0x000100d5   Thumb Code    28  startup_armcm0.o(.text)
    NMI_Handler                              0x000100f1   Thumb Code     2  startup_armcm0.o(.text)
    SVC_Handler                              0x000100f5   Thumb Code     2  startup_armcm0.o(.text)
    PendSV_Handler                           0x000100f7   Thumb Code     2  startup_armcm0.o(.text)
    OTP_IRQn_Handler                         0x00010123   Thumb Code     2  startup_armcm0.o(.text)
    PVD_IRQn_Handler                         0x00010127   Thumb Code     2  startup_armcm0.o(.text)
    __aeabi_uidiv                            0x0001014d   Thumb Code     0  uidiv.o(.text)
    __aeabi_uidivmod                         0x0001014d   Thumb Code    44  uidiv.o(.text)
    __aeabi_idiv                             0x00010179   Thumb Code     0  idiv.o(.text)
    __aeabi_idivmod                          0x00010179   Thumb Code    40  idiv.o(.text)
    __aeabi_memcpy                           0x000101a1   Thumb Code    36  memcpya.o(.text)
    __aeabi_memcpy4                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memcpy8                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memset                           0x000101c5   Thumb Code    14  memseta.o(.text)
    __aeabi_memset4                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memset8                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr                           0x000101d3   Thumb Code     4  memseta.o(.text)
    __aeabi_memclr4                          0x000101d3   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr8                          0x000101d3   Thumb Code     0  memseta.o(.text)
    _memset$wrapper                          0x000101d7   Thumb Code    18  memseta.o(.text)
    __aeabi_fadd                             0x000101e9   Thumb Code   162  fadd.o(.text)
    __aeabi_fsub                             0x0001028b   Thumb Code     8  fadd.o(.text)
    __aeabi_frsub                            0x00010293   Thumb Code     8  fadd.o(.text)
    __aeabi_fmul                             0x0001029b   Thumb Code   122  fmul.o(.text)
    __aeabi_fdiv                             0x00010315   Thumb Code   124  fdiv.o(.text)
    __ARM_scalbnf                            0x00010391   Thumb Code    24  fscalb.o(.text)
    scalbnf                                  0x00010391   Thumb Code     0  fscalb.o(.text)
    __aeabi_dadd                             0x000103a9   Thumb Code   328  dadd.o(.text)
    __aeabi_dsub                             0x000104f1   Thumb Code    12  dadd.o(.text)
    __aeabi_drsub                            0x000104fd   Thumb Code    12  dadd.o(.text)
    __aeabi_i2f                              0x0001050d   Thumb Code    22  fflti.o(.text)
    __aeabi_ui2f                             0x00010523   Thumb Code    14  ffltui.o(.text)
    __aeabi_ui2d                             0x00010531   Thumb Code    24  dfltui.o(.text)
    __aeabi_f2iz                             0x0001054d   Thumb Code    50  ffixi.o(.text)
    __aeabi_f2uiz                            0x0001057f   Thumb Code    40  ffixui.o(.text)
    __aeabi_d2iz                             0x000105a9   Thumb Code    62  dfixi.o(.text)
    __aeabi_d2uiz                            0x000105f1   Thumb Code    50  dfixui.o(.text)
    __aeabi_f2d                              0x0001062d   Thumb Code    40  f2d.o(.text)
    __aeabi_cfrcmple                         0x00010655   Thumb Code    20  cfrcmple.o(.text)
    __aeabi_uldivmod                         0x00010669   Thumb Code    96  uldiv.o(.text)
    __aeabi_llsl                             0x000106c9   Thumb Code    32  llshl.o(.text)
    _ll_shift_l                              0x000106c9   Thumb Code     0  llshl.o(.text)
    __aeabi_llsr                             0x000106e9   Thumb Code    34  llushr.o(.text)
    _ll_ushift_r                             0x000106e9   Thumb Code     0  llushr.o(.text)
    __aeabi_lasr                             0x0001070b   Thumb Code    38  llsshr.o(.text)
    _ll_sshift_r                             0x0001070b   Thumb Code     0  llsshr.o(.text)
    __I$use$fp                               0x00010731   Thumb Code     0  iusefp.o(.text)
    _float_round                             0x00010731   Thumb Code    16  fepilogue.o(.text)
    _float_epilogue                          0x00010741   Thumb Code   114  fepilogue.o(.text)
    _double_round                            0x000107b3   Thumb Code    26  depilogue.o(.text)
    _double_epilogue                         0x000107cd   Thumb Code   164  depilogue.o(.text)
    __aeabi_dmul                             0x00010871   Thumb Code   202  dmul.o(.text)
    __aeabi_ddiv                             0x00010941   Thumb Code   234  ddiv.o(.text)
    __aeabi_d2ulz                            0x00010a31   Thumb Code    54  dfixul.o(.text)
    __aeabi_cdrcmple                         0x00010a71   Thumb Code    38  cdrcmple.o(.text)
    __scatterload                            0x00010a99   Thumb Code    28  init.o(.text)
    __scatterload_rt2                        0x00010a99   Thumb Code     0  init.o(.text)
    __decompress                             0x00010abd   Thumb Code     0  __dczerorl2.o(.text)
    __decompress1                            0x00010abd   Thumb Code    86  __dczerorl2.o(.text)
    ADC_IRQn_Handler                         0x00010b15   Thumb Code    18  irq_redirect .o(i.ADC_IRQn_Handler)
    AP_NRESET_IRQn_Handler                   0x00010b2d   Thumb Code    22  irq_redirect .o(i.AP_NRESET_IRQn_Handler)
    DMA_IRQn_Handler                         0x00010b49   Thumb Code    14  irq_redirect .o(i.DMA_IRQn_Handler)
    EXTI_INT0_IRQn_Handler                   0x00010b5d   Thumb Code    22  irq_redirect .o(i.EXTI_INT0_IRQn_Handler)
    EXTI_INT1_IRQn_Handler                   0x00010b79   Thumb Code    22  irq_redirect .o(i.EXTI_INT1_IRQn_Handler)
    EXTI_INT2_IRQn_Handler                   0x00010b95   Thumb Code    22  irq_redirect .o(i.EXTI_INT2_IRQn_Handler)
    EXTI_INT3_IRQn_Handler                   0x00010bb1   Thumb Code    22  irq_redirect .o(i.EXTI_INT3_IRQn_Handler)
    EXTI_INT4_IRQn_Handler                   0x00010bcd   Thumb Code    22  irq_redirect .o(i.EXTI_INT4_IRQn_Handler)
    EXTI_INT5_IRQn_Handler                   0x00010be9   Thumb Code    22  irq_redirect .o(i.EXTI_INT5_IRQn_Handler)
    EXTI_INT6_IRQn_Handler                   0x00010c05   Thumb Code    22  irq_redirect .o(i.EXTI_INT6_IRQn_Handler)
    EXTI_INT7_IRQn_Handler                   0x00010c21   Thumb Code    22  irq_redirect .o(i.EXTI_INT7_IRQn_Handler)
    FLSCTRL_IRQn_Handler                     0x00010c3d   Thumb Code    14  irq_redirect .o(i.FLSCTRL_IRQn_Handler)
    Gpio_swire_output                        0x00010c51   Thumb Code   110  ap_demo.o(i.Gpio_swire_output)
    HardFault_Handler                        0x00010cc5   Thumb Code    14  irq_redirect .o(i.HardFault_Handler)
    I2C0_IRQn_Handler                        0x00010cd9   Thumb Code    18  irq_redirect .o(i.I2C0_IRQn_Handler)
    I2C1_IRQn_Handler                        0x00010cf1   Thumb Code    18  irq_redirect .o(i.I2C1_IRQn_Handler)
    LCDC_IRQn_Handler                        0x00010d09   Thumb Code    18  irq_redirect .o(i.LCDC_IRQn_Handler)
    LOG_printf                               0x00010d21   Thumb Code    30  tau_log.o(i.LOG_printf)
    MEMC_IRQn_Handler                        0x00010d49   Thumb Code    18  irq_redirect .o(i.MEMC_IRQn_Handler)
    MIPI_RX_IRQn_Handler                     0x00010d61   Thumb Code    18  irq_redirect .o(i.MIPI_RX_IRQn_Handler)
    MIPI_TX_IRQn_Handler                     0x00010d79   Thumb Code    18  irq_redirect .o(i.MIPI_TX_IRQn_Handler)
    PWMDET_IRQn_Handler                      0x00010d91   Thumb Code    22  irq_redirect .o(i.PWMDET_IRQn_Handler)
    S20_Start_init                           0x00010dad   Thumb Code   270  app_tp_transfer.o(i.S20_Start_init)
    SPIM_IRQn_Handler                        0x00010ed1   Thumb Code    22  irq_redirect .o(i.SPIM_IRQn_Handler)
    SPIS_IRQn_Handler                        0x00010eed   Thumb Code    22  irq_redirect .o(i.SPIS_IRQn_Handler)
    SWIRE_IRQn_Handler                       0x00010f09   Thumb Code    22  irq_redirect .o(i.SWIRE_IRQn_Handler)
    SysTick_Handler                          0x00010f25   Thumb Code    18  irq_redirect .o(i.SysTick_Handler)
    TIMER0_IRQn_Handler                      0x00010f3d   Thumb Code    18  irq_redirect .o(i.TIMER0_IRQn_Handler)
    TIMER1_IRQn_Handler                      0x00010f55   Thumb Code    18  irq_redirect .o(i.TIMER1_IRQn_Handler)
    TIMER2_IRQn_Handler                      0x00010f6d   Thumb Code    18  irq_redirect .o(i.TIMER2_IRQn_Handler)
    TIMER3_IRQn_Handler                      0x00010f85   Thumb Code    18  irq_redirect .o(i.TIMER3_IRQn_Handler)
    UART_DisableDma                          0x00010f9d   Thumb Code     2  drv_uart.o(i.UART_DisableDma)
    UART_GetInstance                         0x00010f9f   Thumb Code     4  drv_uart.o(i.UART_GetInstance)
    UART_IRQ_Handle                          0x00010fa5   Thumb Code    20  drv_uart.o(i.UART_IRQ_Handle)
    UART_IRQn_Handler                        0x00010fc1   Thumb Code    18  irq_redirect .o(i.UART_IRQn_Handler)
    UART_ResetRxFIFO                         0x00010fd9   Thumb Code    32  drv_uart.o(i.UART_ResetRxFIFO)
    __scatterload_null                       0x00010ffd   Thumb Code     2  handlers.o(i.__scatterload_null)
    screen_reg_start_data_size               0x00010ffe   Data           1  app_tp_for_custom_s8.o(.constdata)
    s_RAM_CK                                 0x00011000   Data          20  drv_common.o(.ARM.__at_0x11000)
    UART_SetBaudRate                         0x00011015   Thumb Code    72  drv_uart.o(i.UART_SetBaudRate)
    UART_SwitchSCLK                          0x0001105d   Thumb Code    26  drv_uart.o(i.UART_SwitchSCLK)
    UART_TransferHandleIRQ                   0x00011077   Thumb Code   308  drv_uart.o(i.UART_TransferHandleIRQ)
    UART_WriteBlocking                       0x000111ab   Thumb Code    26  drv_uart.o(i.UART_WriteBlocking)
    UART_init                                0x000111c5   Thumb Code   182  drv_uart.o(i.UART_init)
    VIDC_IRQn_Handler                        0x00011281   Thumb Code    18  irq_redirect .o(i.VIDC_IRQn_Handler)
    VPRE_IRQn_Handler                        0x00011299   Thumb Code    18  irq_redirect .o(i.VPRE_IRQn_Handler)
    WDG_IRQn_Handler                         0x000112b1   Thumb Code    18  irq_redirect .o(i.WDG_IRQn_Handler)
    __0printf                                0x000112c9   Thumb Code    24  printfa.o(i.__0printf)
    __1printf                                0x000112c9   Thumb Code     0  printfa.o(i.__0printf)
    __2printf                                0x000112c9   Thumb Code     0  printfa.o(i.__0printf)
    __c89printf                              0x000112c9   Thumb Code     0  printfa.o(i.__0printf)
    printf                                   0x000112c9   Thumb Code     0  printfa.o(i.__0printf)
    __0vsprintf                              0x000112e9   Thumb Code    30  printfa.o(i.__0vsprintf)
    __1vsprintf                              0x000112e9   Thumb Code     0  printfa.o(i.__0vsprintf)
    __2vsprintf                              0x000112e9   Thumb Code     0  printfa.o(i.__0vsprintf)
    __c89vsprintf                            0x000112e9   Thumb Code     0  printfa.o(i.__0vsprintf)
    vsprintf                                 0x000112e9   Thumb Code     0  printfa.o(i.__0vsprintf)
    __ARM_clz                                0x0001130d   Thumb Code    46  depilogue.o(i.__ARM_clz)
    __ARM_common_switch8                     0x0001133b   Thumb Code    26  ap_demo.o(i.__ARM_common_switch8)
    __scatterload_copy                       0x000113c9   Thumb Code    14  handlers.o(i.__scatterload_copy)
    __scatterload_zeroinit                   0x000113d7   Thumb Code    14  handlers.o(i.__scatterload_zeroinit)
    ap_demo                                  0x00013031   Thumb Code   280  ap_demo.o(i.ap_demo)
    ap_tp_calibration                        0x0001379d   Thumb Code   170  app_tp_transfer.o(i.ap_tp_calibration)
    ap_tp_scan_point_init                    0x0001384d   Thumb Code    24  app_tp_transfer.o(i.ap_tp_scan_point_init)
    ap_tp_scan_point_record_event            0x00013869   Thumb Code   150  app_tp_transfer.o(i.ap_tp_scan_point_record_event)
    ap_tp_scan_point_record_event_exec       0x00013905   Thumb Code    50  app_tp_transfer.o(i.ap_tp_scan_point_record_event_exec)
    ap_tp_simulate_finger_release_event      0x00013955   Thumb Code    44  app_tp_transfer.o(i.ap_tp_simulate_finger_release_event)
    ap_tp_system_softReset                   0x00013989   Thumb Code    58  app_tp_transfer.o(i.ap_tp_system_softReset)
    app_AP_NRESET_IRQn_Handler               0x000139c9   Thumb Code    32  drv_gpio.o(i.app_AP_NRESET_IRQn_Handler)
    app_EXTI_INT0_IRQn_Handler               0x000139ed   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler)
    app_EXTI_INT1_IRQn_Handler               0x00013a09   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler)
    app_EXTI_INT2_IRQn_Handler               0x00013a25   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler)
    app_EXTI_INT3_IRQn_Handler               0x00013a41   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler)
    app_EXTI_INT4_IRQn_Handler               0x00013a5d   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler)
    app_EXTI_INT5_IRQn_Handler               0x00013a79   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler)
    app_EXTI_INT6_IRQn_Handler               0x00013a95   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler)
    app_EXTI_INT7_IRQn_Handler               0x00013ab1   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler)
    app_HardFault_Handler                    0x00013acd   Thumb Code    12  drv_common.o(i.app_HardFault_Handler)
    app_I2C0_IRQn_Handler                    0x00013b15   Thumb Code     8  drv_i2c_slave.o(i.app_I2C0_IRQn_Handler)
    app_I2C1_IRQn_Handler                    0x00013b25   Thumb Code     8  drv_i2c_master.o(i.app_I2C1_IRQn_Handler)
    app_LCDC_IRQn_Handler                    0x00013b35   Thumb Code    98  hal_internal_vsync.o(i.app_LCDC_IRQn_Handler)
    app_MEMC_IRQn_Handler                    0x00013c15   Thumb Code    92  drv_memc.o(i.app_MEMC_IRQn_Handler)
    app_MIPI_RX_IRQn_Handler                 0x00013c75   Thumb Code   232  drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler)
    app_MIPI_TX_IRQn_Handler                 0x00013f0d   Thumb Code    56  drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler)
    app_PWMDET_IRQn_Handler                  0x00013fad   Thumb Code    62  drv_pwm.o(i.app_PWMDET_IRQn_Handler)
    app_SPIM_IRQn_Handler                    0x00013ff5   Thumb Code    22  drv_spi_master.o(i.app_SPIM_IRQn_Handler)
    app_SPIS_IRQn_Handler                    0x00014015   Thumb Code   500  hal_spi_slave.o(i.app_SPIS_IRQn_Handler)
    app_SWIRE_IRQn_Handler                   0x00014215   Thumb Code    28  drv_swire.o(i.app_SWIRE_IRQn_Handler)
    app_SysTick_Handler                      0x00014235   Thumb Code    20  drv_common.o(i.app_SysTick_Handler)
    app_TIMER0_IRQn_Handler                  0x0001424d   Thumb Code    10  drv_timer.o(i.app_TIMER0_IRQn_Handler)
    app_TIMER1_IRQn_Handler                  0x00014257   Thumb Code    10  drv_timer.o(i.app_TIMER1_IRQn_Handler)
    app_TIMER2_IRQn_Handler                  0x00014261   Thumb Code    10  drv_timer.o(i.app_TIMER2_IRQn_Handler)
    app_TIMER3_IRQn_Handler                  0x0001426b   Thumb Code    10  drv_timer.o(i.app_TIMER3_IRQn_Handler)
    app_UART_IRQn_Handler                    0x00014275   Thumb Code     8  drv_uart.o(i.app_UART_IRQn_Handler)
    app_VIDC_IRQn_Handler                    0x0001427d   Thumb Code   190  hal_internal_vsync.o(i.app_VIDC_IRQn_Handler)
    app_VPRE_IRQn_Handler                    0x00014361   Thumb Code   544  hal_internal_vsync.o(i.app_VPRE_IRQn_Handler)
    app_WDG_IRQn_Handler                     0x000145e5   Thumb Code    52  drv_wdg.o(i.app_WDG_IRQn_Handler)
    app_dma_irq_handler                      0x0001461d   Thumb Code     8  drv_dma.o(i.app_dma_irq_handler)
    app_fls_ctrl_Handler                     0x00014625   Thumb Code    38  norflash.o(i.app_fls_ctrl_Handler)
    app_tp_I2C_init                          0x00014655   Thumb Code    26  app_tp_transfer.o(i.app_tp_I2C_init)
    app_tp_calibration_exec                  0x00014679   Thumb Code    30  ap_demo.o(i.app_tp_calibration_exec)
    app_tp_init                              0x000146e1   Thumb Code    60  app_tp_transfer.o(i.app_tp_init)
    app_tp_m_transfer_complate               0x00014749   Thumb Code     8  app_tp_transfer.o(i.app_tp_m_transfer_complate)
    app_tp_phone_analysis_data               0x00014759   Thumb Code   980  app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data)
    app_tp_phone_clear_reset_on              0x00014b69   Thumb Code     8  app_tp_transfer.o(i.app_tp_phone_clear_reset_on)
    app_tp_s_read                            0x00014b75   Thumb Code     8  app_tp_transfer.o(i.app_tp_s_read)
    app_tp_s_write                           0x00014b7d   Thumb Code     8  app_tp_transfer.o(i.app_tp_s_write)
    app_tp_screen_analysis_int               0x00014b85   Thumb Code   704  app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int)
    app_tp_screen_init                       0x00014e51   Thumb Code    42  app_tp_transfer.o(i.app_tp_screen_init)
    app_tp_transfer_screen_int               0x00014f39   Thumb Code   420  app_tp_transfer.o(i.app_tp_transfer_screen_int)
    app_tp_transfer_screen_start             0x00015119   Thumb Code    18  app_tp_transfer.o(i.app_tp_transfer_screen_start)
    blue_change_ccm                          0x00015131   Thumb Code    54  ap_demo.o(i.blue_change_ccm)
    board_Init                               0x00015169   Thumb Code    24  board.o(i.board_Init)
    ceil                                     0x00015371   Thumb Code   180  ceil.o(i.ceil)
    dcs_packet_fifo_alloc                    0x00015491   Thumb Code    80  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    dcs_packet_fifo_init                     0x000154e9   Thumb Code    18  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    dcs_packet_free_fifo_header              0x00015501   Thumb Code    60  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    dcs_packet_get_fifo_header               0x00015545   Thumb Code    26  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    delayMs                                  0x00015585   Thumb Code    24  tau_delay.o(i.delayMs)
    delayUs                                  0x0001559d   Thumb Code    34  tau_delay.o(i.delayUs)
    drv_ap_rst_trig_edge_detect              0x00015655   Thumb Code    46  drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect)
    drv_chip_info_get_version                0x0001568d   Thumb Code     6  drv_chip_info.o(i.drv_chip_info_get_version)
    drv_chip_info_init                       0x00015699   Thumb Code   158  drv_chip_info.o(i.drv_chip_info_init)
    drv_chip_rx_info_check                   0x00015749   Thumb Code    54  drv_chip_info.o(i.drv_chip_rx_info_check)
    drv_chip_rx_init_done                    0x000157a5   Thumb Code    16  drv_chip_info.o(i.drv_chip_rx_init_done)
    drv_common_enable_systick                0x000157b9   Thumb Code    70  drv_common.o(i.drv_common_enable_systick)
    drv_common_system_init                   0x00015811   Thumb Code    34  drv_common.o(i.drv_common_system_init)
    drv_crgu_config_reset_modules            0x00015841   Thumb Code    10  drv_crgu.o(i.drv_crgu_config_reset_modules)
    drv_crgu_set_ahb_pre_div                 0x00015851   Thumb Code    14  drv_crgu.o(i.drv_crgu_set_ahb_pre_div)
    drv_crgu_set_ahb_src                     0x00015865   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_ahb_src)
    drv_crgu_set_clock                       0x00015879   Thumb Code    26  drv_crgu.o(i.drv_crgu_set_clock)
    drv_crgu_set_dpi_mux_src                 0x00015899   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dpi_mux_src)
    drv_crgu_set_dpi_pre_div                 0x000158ad   Thumb Code    18  drv_crgu.o(i.drv_crgu_set_dpi_pre_div)
    drv_crgu_set_dpi_pre_src                 0x000158c5   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dpi_pre_src)
    drv_crgu_set_dsc_core_div                0x000158d9   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dsc_core_div)
    drv_crgu_set_dsco_src                    0x000158ed   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dsco_src)
    drv_crgu_set_dsco_src_div                0x00015901   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dsco_src_div)
    drv_crgu_set_fb_div                      0x00015915   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_fb_div)
    drv_crgu_set_fb_src                      0x00015929   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_fb_src)
    drv_crgu_set_lcdc_div                    0x0001593d   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_lcdc_div)
    drv_crgu_set_lcdc_src                    0x00015951   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_lcdc_src)
    drv_crgu_set_mipi_cfg_src                0x00015965   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_mipi_cfg_src)
    drv_crgu_set_mipi_ref_src                0x00015979   Thumb Code    18  drv_crgu.o(i.drv_crgu_set_mipi_ref_src)
    drv_crgu_set_reset                       0x00015991   Thumb Code    20  drv_crgu.o(i.drv_crgu_set_reset)
    drv_crgu_set_rxbr_div                    0x000159a9   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_rxbr_div)
    drv_crgu_set_rxbr_src                    0x000159bd   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_rxbr_src)
    drv_crgu_set_vidc_src                    0x000159d1   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_vidc_src)
    drv_dma_clear_flag                       0x000159e5   Thumb Code    22  drv_dma.o(i.drv_dma_clear_flag)
    drv_dma_create_handle                    0x00015a01   Thumb Code    18  drv_dma.o(i.drv_dma_create_handle)
    drv_dma_disenable_channel                0x00015a19   Thumb Code    18  drv_dma.o(i.drv_dma_disenable_channel)
    drv_dma_enable_channel                   0x00015a31   Thumb Code    18  drv_dma.o(i.drv_dma_enable_channel)
    drv_dma_enable_channel_interrupts        0x00015a49   Thumb Code    42  drv_dma.o(i.drv_dma_enable_channel_interrupts)
    drv_dma_enable_cycle                     0x00015a7d   Thumb Code    42  drv_dma.o(i.drv_dma_enable_cycle)
    drv_dma_get_channel_flag                 0x00015aad   Thumb Code    14  drv_dma.o(i.drv_dma_get_channel_flag)
    drv_dma_irq_handler                      0x00015ac1   Thumb Code   118  drv_dma.o(i.drv_dma_irq_handler)
    drv_dma_prepar_transfer                  0x00015b3d   Thumb Code    18  drv_dma.o(i.drv_dma_prepar_transfer)
    drv_dma_set_burst                        0x00015b55   Thumb Code    24  drv_dma.o(i.drv_dma_set_burst)
    drv_dma_set_callback                     0x00015b71   Thumb Code     6  drv_dma.o(i.drv_dma_set_callback)
    drv_dma_set_transfer                     0x00015b79   Thumb Code    62  drv_dma.o(i.drv_dma_set_transfer)
    drv_dsc_dec_convert_pps_rc_parameter     0x00015bbd   Thumb Code    54  drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter)
    drv_dsc_dec_disable                      0x00015bf3   Thumb Code    12  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    drv_dsc_dec_enable                       0x00015c01   Thumb Code   146  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    drv_dsc_dec_get_nslc                     0x00015cb5   Thumb Code    10  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    drv_dsc_dec_set_u8_pps                   0x00015cbf   Thumb Code    40  drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps)
    drv_dsi_rx_calc_ipi_tx_delay             0x00015ce9   Thumb Code   244  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    drv_dsi_rx_enable_irq                    0x00015ded   Thumb Code    58  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    drv_dsi_rx_get_compression_en            0x00015e99   Thumb Code     8  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    drv_dsi_rx_get_max_ret_size              0x00015ea1   Thumb Code     6  drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size)
    drv_dsi_rx_power_up                      0x00015ea7   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    drv_dsi_rx_set_ctrl_cfg                  0x00015eb5   Thumb Code    28  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    drv_dsi_rx_set_ddi_cfg                   0x00015ed1   Thumb Code    16  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    drv_dsi_rx_set_inten                     0x00015ee1   Thumb Code     4  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    drv_dsi_rx_set_ipi_cfg                   0x00015ee5   Thumb Code    16  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    drv_dsi_rx_set_resp_cnt                  0x00015ef5   Thumb Code    38  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    drv_dsi_rx_set_up_phy                    0x00015f1d   Thumb Code   138  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    drv_dsi_rx_shut_down                     0x00015fad   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    drv_dsi_tx_command_header                0x00015fbb   Thumb Code    20  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    drv_dsi_tx_command_mode_cfg              0x00015fcf   Thumb Code   108  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    drv_dsi_tx_command_put_payload           0x0001603b   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    drv_dsi_tx_config_eotp                   0x0001603f   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    drv_dsi_tx_config_int                    0x00016057   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    drv_dsi_tx_dpi_lpcmd_time                0x0001605f   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    drv_dsi_tx_dpi_mode                      0x00016067   Thumb Code    10  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    drv_dsi_tx_dpi_polarity                  0x00016071   Thumb Code    36  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    drv_dsi_tx_get_cmd_status                0x00016095   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    drv_dsi_tx_mode                          0x00016099   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    drv_dsi_tx_phy_clock_lane_auto_lp        0x0001609d   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    drv_dsi_tx_phy_clock_lane_req_hs         0x000160b5   Thumb Code    26  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    drv_dsi_tx_phy_lane_mode                 0x000160cf   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    drv_dsi_tx_phy_status_ready              0x000160db   Thumb Code   100  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    drv_dsi_tx_phy_status_stopstate          0x0001613f   Thumb Code    62  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    drv_dsi_tx_phy_test_setup                0x0001617d   Thumb Code   228  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    drv_dsi_tx_phy_time_cfg                  0x00016261   Thumb Code    30  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    drv_dsi_tx_powerup                       0x0001627f   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    drv_dsi_tx_response_mode                 0x00016287   Thumb Code    28  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    drv_dsi_tx_set_bta_ack                   0x000162a3   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    drv_dsi_tx_set_esc_div                   0x000162bb   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    drv_dsi_tx_set_int                       0x000162c9   Thumb Code    46  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    drv_dsi_tx_set_time_out_div              0x000162fd   Thumb Code    16  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    drv_dsi_tx_set_video_chunk               0x0001630d   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    drv_dsi_tx_set_video_timing              0x00016315   Thumb Code    34  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    drv_dsi_tx_shutdown                      0x00016337   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    drv_dsi_tx_timeout_cfg                   0x0001633f   Thumb Code    38  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    drv_dsi_tx_video_mode_cfg                0x00016365   Thumb Code   170  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    drv_dsi_tx_video_mode_disable_hact_cmd   0x0001640f   Thumb Code    22  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_disable_hact_cmd)
    drv_dsi_tx_video_mode_set_lp_cmd         0x00016425   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd)
    drv_gpio_get_input_data                  0x0001643d   Thumb Code    20  drv_gpio.o(i.drv_gpio_get_input_data)
    drv_gpio_register_ap_reset_callback      0x00016455   Thumb Code     6  drv_gpio.o(i.drv_gpio_register_ap_reset_callback)
    drv_gpio_register_callback               0x00016461   Thumb Code    14  drv_gpio.o(i.drv_gpio_register_callback)
    drv_gpio_set_int                         0x00016475   Thumb Code    62  drv_gpio.o(i.drv_gpio_set_int)
    drv_gpio_set_ioe                         0x000164b9   Thumb Code    26  drv_gpio.o(i.drv_gpio_set_ioe)
    drv_gpio_set_mode0                       0x000164d9   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode0)
    drv_gpio_set_mode1                       0x000164e9   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode1)
    drv_gpio_set_mode2                       0x000164f9   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode2)
    drv_gpio_set_mode3                       0x00016509   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode3)
    drv_gpio_set_pull_state                  0x00016539   Thumb Code   298  drv_gpio.o(i.drv_gpio_set_pull_state)
    drv_i2c_clear_m_it_pending_bit           0x00016669   Thumb Code    86  drv_i2c_master.o(i.drv_i2c_clear_m_it_pending_bit)
    drv_i2c_clear_s_it_pending_bit           0x000166c9   Thumb Code    84  drv_i2c_slave.o(i.drv_i2c_clear_s_it_pending_bit)
    drv_i2c_dma_init                         0x00016759   Thumb Code   146  drv_i2c_dma.o(i.drv_i2c_dma_init)
    drv_i2c_enable_rx_dma                    0x00016805   Thumb Code    26  drv_i2c_dma.o(i.drv_i2c_enable_rx_dma)
    drv_i2c_enable_tx_dma                    0x0001681f   Thumb Code    24  drv_i2c_dma.o(i.drv_i2c_enable_tx_dma)
    drv_i2c_m_enable_intr                    0x00016839   Thumb Code    42  drv_i2c_master.o(i.drv_i2c_m_enable_intr)
    drv_i2c_m_set_callback                   0x00016871   Thumb Code     6  drv_i2c_master.o(i.drv_i2c_m_set_callback)
    drv_i2c_master_init                      0x0001687d   Thumb Code   118  drv_i2c_master.o(i.drv_i2c_master_init)
    drv_i2c_master_read_dma                  0x00016909   Thumb Code   114  drv_i2c_dma.o(i.drv_i2c_master_read_dma)
    drv_i2c_master_write_dma                 0x00016985   Thumb Code    60  drv_i2c_dma.o(i.drv_i2c_master_write_dma)
    drv_i2c_s_enable_intr                    0x000169f5   Thumb Code    40  drv_i2c_slave.o(i.drv_i2c_s_enable_intr)
    drv_i2c_s_get_fifo_status                0x00016a29   Thumb Code    22  drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status)
    drv_i2c_s_set_callback                   0x00016a45   Thumb Code     6  drv_i2c_slave.o(i.drv_i2c_s_set_callback)
    drv_i2c_s_write_data                     0x00016a51   Thumb Code    26  drv_i2c_slave.o(i.drv_i2c_s_write_data)
    drv_i2c_set_dma_irq_callback             0x00016a71   Thumb Code    62  drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback)
    drv_i2c_slave_init                       0x00016ac1   Thumb Code    60  drv_i2c_slave.o(i.drv_i2c_slave_init)
    drv_i2c_slave_write_dma                  0x00016b05   Thumb Code    30  drv_i2c_dma.o(i.drv_i2c_slave_write_dma)
    drv_lcdc_config_420_to_444_mode          0x00016b29   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_config_420_to_444_mode)
    drv_lcdc_config_bypass                   0x00016b41   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_config_bypass)
    drv_lcdc_config_cbcr                     0x00016b59   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_config_cbcr)
    drv_lcdc_config_ccm                      0x00016b71   Thumb Code    48  drv_lcdc.o(i.drv_lcdc_config_ccm)
    drv_lcdc_config_disp_mode                0x00016ba1   Thumb Code    22  drv_lcdc.o(i.drv_lcdc_config_disp_mode)
    drv_lcdc_config_dpi_polarity             0x00016bb7   Thumb Code    36  drv_lcdc.o(i.drv_lcdc_config_dpi_polarity)
    drv_lcdc_config_dpi_timing               0x00016bdb   Thumb Code    38  drv_lcdc.o(i.drv_lcdc_config_dpi_timing)
    drv_lcdc_config_endianness               0x00016c01   Thumb Code    22  drv_lcdc.o(i.drv_lcdc_config_endianness)
    drv_lcdc_config_horiz_flip               0x00016c17   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_config_horiz_flip)
    drv_lcdc_config_input_size               0x00016c37   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_config_input_size)
    drv_lcdc_config_int                      0x00016c43   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_config_int)
    drv_lcdc_config_int_single               0x00016c61   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_int_single)
    drv_lcdc_config_overwrite                0x00016c83   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_overwrite)
    drv_lcdc_config_overwrite_rgb            0x00016ca5   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    drv_lcdc_config_partial_display_area     0x00016cb1   Thumb Code    26  drv_lcdc.o(i.drv_lcdc_config_partial_display_area)
    drv_lcdc_config_partial_display_enable   0x00016ccb   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_partial_display_enable)
    drv_lcdc_config_src_parameter            0x00016ced   Thumb Code   114  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    drv_lcdc_config_thresh                   0x00016d5f   Thumb Code     8  drv_lcdc.o(i.drv_lcdc_config_thresh)
    drv_lcdc_config_upscaler                 0x00016d67   Thumb Code    96  drv_lcdc.o(i.drv_lcdc_config_upscaler)
    drv_lcdc_config_yuv420_threshold         0x00016dc7   Thumb Code    10  drv_lcdc.o(i.drv_lcdc_config_yuv420_threshold)
    drv_lcdc_ctrl_flow                       0x00016dd1   Thumb Code    18  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    drv_lcdc_enable_shadow_reg               0x00016de3   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    drv_lcdc_set_int                         0x00016e05   Thumb Code    46  drv_lcdc.o(i.drv_lcdc_set_int)
    drv_lcdc_start                           0x00016e39   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_start)
    drv_lcdc_update_shadow_reg               0x00016e59   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_update_shadow_reg)
    drv_memc_bypass_fifo_empty               0x00016e65   Thumb Code    16  drv_memc.o(i.drv_memc_bypass_fifo_empty)
    drv_memc_clear_status                    0x00016e75   Thumb Code    12  drv_memc.o(i.drv_memc_clear_status)
    drv_memc_enable_irq                      0x00016e81   Thumb Code    58  drv_memc.o(i.drv_memc_enable_irq)
    drv_memc_gen_a_tear_signal               0x00016ec1   Thumb Code    12  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    drv_memc_get_status                      0x00016ecd   Thumb Code    18  drv_memc.o(i.drv_memc_get_status)
    drv_memc_rate_transfer_sel               0x00016edf   Thumb Code    16  drv_memc.o(i.drv_memc_rate_transfer_sel)
    drv_memc_sel_vsync                       0x00016eef   Thumb Code    14  drv_memc.o(i.drv_memc_sel_vsync)
    drv_memc_set_data_mode                   0x00016efd   Thumb Code    12  drv_memc.o(i.drv_memc_set_data_mode)
    drv_memc_set_tear_hwclr                  0x00016f09   Thumb Code    16  drv_memc.o(i.drv_memc_set_tear_hwclr)
    drv_memc_set_tear_mode                   0x00016f19   Thumb Code    14  drv_memc.o(i.drv_memc_set_tear_mode)
    drv_memc_set_tear_waveform               0x00016f29   Thumb Code    28  drv_memc.o(i.drv_memc_set_tear_waveform)
    drv_memc_set_yuv420_cfg                  0x00016f4d   Thumb Code    16  drv_memc.o(i.drv_memc_set_yuv420_cfg)
    drv_param_get_picture_quality_setting    0x00016f5d   Thumb Code    12  drv_param_init.o(i.drv_param_get_picture_quality_setting)
    drv_param_init_get_ccm                   0x00016f6d   Thumb Code     4  drv_param_init.o(i.drv_param_init_get_ccm)
    drv_param_init_get_scld_filter_h         0x00016f75   Thumb Code    12  drv_param_init.o(i.drv_param_init_get_scld_filter_h)
    drv_param_init_get_scld_filter_v         0x00016f89   Thumb Code    12  drv_param_init.o(i.drv_param_init_get_scld_filter_v)
    drv_param_init_get_sclu_filter_h         0x00016f9d   Thumb Code     4  drv_param_init.o(i.drv_param_init_get_sclu_filter_h)
    drv_param_init_get_sclu_filter_v         0x00016fa5   Thumb Code     4  drv_param_init.o(i.drv_param_init_get_sclu_filter_v)
    drv_param_init_set_ccm                   0x00016fad   Thumb Code    14  drv_param_init.o(i.drv_param_init_set_ccm)
    drv_param_p2r_filter_init                0x00016fc1   Thumb Code    54  drv_param_init.o(i.drv_param_p2r_filter_init)
    drv_param_yuv420_filter_init             0x00016ffd   Thumb Code    48  drv_param_init.o(i.drv_param_yuv420_filter_init)
    drv_phy_get_pll_para                     0x00017031   Thumb Code    88  drv_phy_common.o(i.drv_phy_get_pll_para)
    drv_phy_get_rate_para                    0x00017091   Thumb Code    76  drv_phy_common.o(i.drv_phy_get_rate_para)
    drv_phy_test_clear                       0x000170e5   Thumb Code    16  drv_phy_common.o(i.drv_phy_test_clear)
    drv_phy_test_lock                        0x000170f5   Thumb Code    24  drv_phy_common.o(i.drv_phy_test_lock)
    drv_phy_test_write_1_byte                0x0001710d   Thumb Code    32  drv_phy_common.o(i.drv_phy_test_write_1_byte)
    drv_phy_test_write_2_byte                0x0001712d   Thumb Code    38  drv_phy_common.o(i.drv_phy_test_write_2_byte)
    drv_phy_test_write_code                  0x00017153   Thumb Code    30  drv_phy_common.o(i.drv_phy_test_write_code)
    drv_pwr_set_cp_mode                      0x00017191   Thumb Code    26  drv_pwr.o(i.drv_pwr_set_cp_mode)
    drv_pwr_set_pvd_mode                     0x000171b1   Thumb Code    24  drv_pwr.o(i.drv_pwr_set_pvd_mode)
    drv_pwr_set_system_clk_src               0x000171cd   Thumb Code    36  drv_pwr.o(i.drv_pwr_set_system_clk_src)
    drv_rxbr_clear_pkt_buffer                0x00017243   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    drv_rxbr_clear_status                    0x00017249   Thumb Code     4  drv_rxbr.o(i.drv_rxbr_clear_status)
    drv_rxbr_enable_irq                      0x0001724d   Thumb Code    58  drv_rxbr.o(i.drv_rxbr_enable_irq)
    drv_rxbr_frame_drop_cfg                  0x0001728d   Thumb Code     8  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    drv_rxbr_get_clk                         0x00017295   Thumb Code    44  drv_rxbr.o(i.drv_rxbr_get_clk)
    drv_rxbr_get_col_addr                    0x000172d1   Thumb Code     4  drv_rxbr.o(i.drv_rxbr_get_col_addr)
    drv_rxbr_get_cur_hline_rcv_cnt           0x000172d5   Thumb Code     8  drv_rxbr.o(i.drv_rxbr_get_cur_hline_rcv_cnt)
    drv_rxbr_get_hline_rcv_cfg               0x000172dd   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_get_hline_rcv_cfg)
    drv_rxbr_get_page_addr                   0x000172ff   Thumb Code     4  drv_rxbr.o(i.drv_rxbr_get_page_addr)
    drv_rxbr_hline_rcv0_cfg                  0x00017327   Thumb Code    12  drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg)
    drv_rxbr_hline_rcv_cfg                   0x00017333   Thumb Code     8  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    drv_rxbr_set_ack_pkt_header              0x0001733b   Thumb Code    20  drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header)
    drv_rxbr_set_cmd_filter                  0x0001734f   Thumb Code   204  drv_rxbr.o(i.drv_rxbr_set_cmd_filter)
    drv_rxbr_set_color_format                0x0001741b   Thumb Code    20  drv_rxbr.o(i.drv_rxbr_set_color_format)
    drv_rxbr_set_inten                       0x0001742f   Thumb Code    20  drv_rxbr.o(i.drv_rxbr_set_inten)
    drv_rxbr_set_usr_cfg                     0x00017443   Thumb Code    34  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    drv_rxbr_set_usr_col                     0x00017465   Thumb Code     8  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    drv_rxbr_set_usr_row                     0x0001746d   Thumb Code     8  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    drv_spi_m_read_data                      0x00017475   Thumb Code    28  drv_spi_master.o(i.drv_spi_m_read_data)
    drv_swire_set_int                        0x00017495   Thumb Code    64  drv_swire.o(i.drv_swire_set_int)
    drv_swire_set_power_down                 0x000174dd   Thumb Code    24  drv_swire.o(i.drv_swire_set_power_down)
    drv_sys_cfg_clear_all_int                0x000174f9   Thumb Code     8  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    drv_sys_cfg_clear_pending                0x00017505   Thumb Code    32  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    drv_sys_cfg_sel_ap_rst_lvl_trig          0x0001752d   Thumb Code    18  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig)
    drv_sys_cfg_sel_ap_rst_trig              0x00017545   Thumb Code    22  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig)
    drv_sys_cfg_sel_gpio_group               0x00017561   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group)
    drv_sys_cfg_sel_int_trig                 0x00017585   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig)
    drv_sys_cfg_set_dma_rx_req               0x000175a9   Thumb Code    10  drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req)
    drv_sys_cfg_set_dma_tx_req               0x000175b9   Thumb Code    10  drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req)
    drv_sys_cfg_set_int                      0x000175c9   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    drv_timer_enable                         0x00017607   Thumb Code    32  drv_timer.o(i.drv_timer_enable)
    drv_timer_get_instance                   0x00017629   Thumb Code    10  drv_timer.o(i.drv_timer_get_instance)
    drv_timer_get_prescaler                  0x00017639   Thumb Code    12  drv_timer.o(i.drv_timer_get_prescaler)
    drv_timer_register_callback              0x00017685   Thumb Code    14  drv_timer.o(i.drv_timer_register_callback)
    drv_timer_set_compare_val                0x00017699   Thumb Code    16  drv_timer.o(i.drv_timer_set_compare_val)
    drv_timer_set_int                        0x000176a9   Thumb Code    68  drv_timer.o(i.drv_timer_set_int)
    drv_timer_set_prescaler                  0x000176f1   Thumb Code    36  drv_timer.o(i.drv_timer_set_prescaler)
    drv_tx_phy_test_enter                    0x00017723   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    drv_tx_phy_test_exit                     0x0001773f   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    drv_vidc_clear_irq                       0x00017791   Thumb Code     8  drv_vidc.o(i.drv_vidc_clear_irq)
    drv_vidc_enable                          0x00017799   Thumb Code    24  drv_vidc.o(i.drv_vidc_enable)
    drv_vidc_enable_irq                      0x000177b1   Thumb Code    58  drv_vidc.o(i.drv_vidc_enable_irq)
    drv_vidc_get_int_source                  0x000177f1   Thumb Code    38  drv_vidc.o(i.drv_vidc_get_int_source)
    drv_vidc_module_enable                   0x00017819   Thumb Code    62  drv_vidc.o(i.drv_vidc_module_enable)
    drv_vidc_reset                           0x0001785d   Thumb Code     6  drv_vidc.o(i.drv_vidc_reset)
    drv_vidc_set_dst_parameter               0x00017863   Thumb Code    92  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    drv_vidc_set_enh_chr                     0x000178bf   Thumb Code    14  drv_vidc.o(i.drv_vidc_set_enh_chr)
    drv_vidc_set_enh_chr2                    0x000178cd   Thumb Code    18  drv_vidc.o(i.drv_vidc_set_enh_chr2)
    drv_vidc_set_enh_lum                     0x000178df   Thumb Code    14  drv_vidc.o(i.drv_vidc_set_enh_lum)
    drv_vidc_set_gain                        0x000178ed   Thumb Code    48  drv_vidc.o(i.drv_vidc_set_gain)
    drv_vidc_set_irqen                       0x0001791d   Thumb Code    20  drv_vidc.o(i.drv_vidc_set_irqen)
    drv_vidc_set_p2r_hcoef0                  0x00017931   Thumb Code     8  drv_vidc.o(i.drv_vidc_set_p2r_hcoef0)
    drv_vidc_set_p2r_hcoef1                  0x00017939   Thumb Code     8  drv_vidc.o(i.drv_vidc_set_p2r_hcoef1)
    drv_vidc_set_p2r_hinitb                  0x00017941   Thumb Code    40  drv_vidc.o(i.drv_vidc_set_p2r_hinitb)
    drv_vidc_set_p2r_hinitr                  0x00017969   Thumb Code    40  drv_vidc.o(i.drv_vidc_set_p2r_hinitr)
    drv_vidc_set_p2r_step                    0x00017991   Thumb Code     8  drv_vidc.o(i.drv_vidc_set_p2r_step)
    drv_vidc_set_pu_ctrl                     0x00017999   Thumb Code    32  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    drv_vidc_set_pu_scld                     0x000179b9   Thumb Code    14  drv_vidc.o(i.drv_vidc_set_pu_scld)
    drv_vidc_set_scld_hcoef0                 0x000179c7   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    drv_vidc_set_scld_hcoef1                 0x000179d1   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    drv_vidc_set_scld_step                   0x000179db   Thumb Code    18  drv_vidc.o(i.drv_vidc_set_scld_step)
    drv_vidc_set_scld_vcoef0                 0x000179ed   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    drv_vidc_set_scld_vcoef1                 0x000179f7   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    drv_vidc_set_sclu_hcoef0c                0x00017a01   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_sclu_hcoef0c)
    drv_vidc_set_sclu_hcoef0y                0x00017a0b   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_sclu_hcoef0y)
    drv_vidc_set_sclu_hcoef1c                0x00017a15   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_sclu_hcoef1c)
    drv_vidc_set_sclu_hcoef1y                0x00017a1f   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_sclu_hcoef1y)
    drv_vidc_set_sclu_vcoef0c                0x00017a29   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_sclu_vcoef0c)
    drv_vidc_set_sclu_vcoef0y                0x00017a33   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_sclu_vcoef0y)
    drv_vidc_set_sclu_vcoef1c                0x00017a3d   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_sclu_vcoef1c)
    drv_vidc_set_sclu_vcoef1y                0x00017a47   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_sclu_vcoef1y)
    drv_vidc_set_src_parameter               0x00017a51   Thumb Code    32  drv_vidc.o(i.drv_vidc_set_src_parameter)
    drv_vidc_set_y4t2_hcoef0                 0x00017a75   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_y4t2_hcoef0)
    drv_vidc_set_y4t2_hcoef1                 0x00017a7f   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_y4t2_hcoef1)
    drv_vidc_set_y4t2_vcoef0                 0x00017a89   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_y4t2_vcoef0)
    drv_vidc_set_y4t2_vcoef1                 0x00017a93   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_y4t2_vcoef1)
    drv_wdg_clear_counter                    0x00017a9d   Thumb Code    12  drv_wdg.o(i.drv_wdg_clear_counter)
    drv_wdg_set_int                          0x00017acd   Thumb Code    48  drv_wdg.o(i.drv_wdg_set_int)
    fls_clear_irq_status                     0x00017b01   Thumb Code     6  drv_fls.o(i.fls_clear_irq_status)
    fputc                                    0x00017b07   Thumb Code    20  tau_log.o(i.fputc)
    hal_dsi_rx_ctrl_create_handle            0x00017b1d   Thumb Code    42  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    hal_dsi_rx_ctrl_deinit                   0x00017b4d   Thumb Code   148  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit)
    hal_dsi_rx_ctrl_dsc_async_handler        0x00017be9   Thumb Code   122  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler)
    hal_dsi_rx_ctrl_gen_a_tear_signal        0x00017c6d   Thumb Code    32  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal)
    hal_dsi_rx_ctrl_get_max_ret_size         0x00017c95   Thumb Code    30  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size)
    hal_dsi_rx_ctrl_init                     0x00017cbd   Thumb Code    92  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    hal_dsi_rx_ctrl_pre_init_pps             0x000184f1   Thumb Code    56  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    hal_dsi_rx_ctrl_send_ack_cmd             0x0001852d   Thumb Code   212  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd)
    hal_dsi_rx_ctrl_set_cus_sync_line        0x0001861d   Thumb Code    44  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line)
    hal_dsi_rx_ctrl_set_hw_tear_mode         0x00018651   Thumb Code    42  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode)
    hal_dsi_rx_ctrl_set_sw_tear_mode         0x0001872d   Thumb Code    42  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode)
    hal_dsi_rx_ctrl_start                    0x00018761   Thumb Code    46  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    hal_dsi_rx_ctrl_stop                     0x0001879d   Thumb Code    58  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop)
    hal_dsi_rx_ctrl_toggle_resolution        0x000187e5   Thumb Code    28  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    hal_dsi_tx_ctrl_create_handle            0x00018d89   Thumb Code    34  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    hal_dsi_tx_ctrl_deinit                   0x00018db5   Thumb Code    68  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit)
    hal_dsi_tx_ctrl_enter_init_panel_mode    0x00018dfd   Thumb Code    68  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode)
    hal_dsi_tx_ctrl_exit_init_panel_mode     0x00018e49   Thumb Code    30  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode)
    hal_dsi_tx_ctrl_init                     0x00018e6d   Thumb Code   188  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    hal_dsi_tx_ctrl_panel_reset_pin          0x00018f55   Thumb Code    12  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin)
    hal_dsi_tx_ctrl_set_ccm                  0x00018f61   Thumb Code    28  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm)
    hal_dsi_tx_ctrl_set_overwrite_rgb        0x00018f81   Thumb Code    16  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    hal_dsi_tx_ctrl_set_partial_disp         0x00018f95   Thumb Code    12  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp)
    hal_dsi_tx_ctrl_set_partial_disp_area    0x00018fa5   Thumb Code    30  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area)
    hal_dsi_tx_ctrl_start                    0x00018fc9   Thumb Code    84  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    hal_dsi_tx_ctrl_stop                     0x00019029   Thumb Code    54  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop)
    hal_dsi_tx_ctrl_write_array_cmd          0x0001906d   Thumb Code   406  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd)
    hal_dsi_tx_ctrl_write_cmd                0x00019209   Thumb Code   332  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    hal_gpio_ctrl_eint                       0x00019521   Thumb Code    18  hal_gpio.o(i.hal_gpio_ctrl_eint)
    hal_gpio_get_input_data                  0x00019539   Thumb Code    18  hal_gpio.o(i.hal_gpio_get_input_data)
    hal_gpio_init_eint                       0x0001954d   Thumb Code    58  hal_gpio.o(i.hal_gpio_init_eint)
    hal_gpio_init_input                      0x0001958d   Thumb Code    28  hal_gpio.o(i.hal_gpio_init_input)
    hal_gpio_init_output                     0x000195ad   Thumb Code    34  hal_gpio.o(i.hal_gpio_init_output)
    hal_gpio_reg_eint_cb                     0x000195d5   Thumb Code    20  hal_gpio.o(i.hal_gpio_reg_eint_cb)
    hal_gpio_set_ap_reset_int                0x000195ed   Thumb Code    76  hal_gpio.o(i.hal_gpio_set_ap_reset_int)
    hal_gpio_set_mode                        0x0001963d   Thumb Code    90  hal_gpio.o(i.hal_gpio_set_mode)
    hal_gpio_set_output_data                 0x0001969d   Thumb Code     8  hal_gpio.o(i.hal_gpio_set_output_data)
    hal_gpio_set_pull_state                  0x000196a5   Thumb Code    26  hal_gpio.o(i.hal_gpio_set_pull_state)
    hal_i2c_m_dma_init                       0x000196c5   Thumb Code    92  hal_i2c_master.o(i.hal_i2c_m_dma_init)
    hal_i2c_m_dma_read                       0x00019731   Thumb Code    36  hal_i2c_master.o(i.hal_i2c_m_dma_read)
    hal_i2c_m_dma_write                      0x0001975d   Thumb Code    32  hal_i2c_master.o(i.hal_i2c_m_dma_write)
    hal_i2c_m_transfer_complate              0x00019785   Thumb Code    24  hal_i2c_master.o(i.hal_i2c_m_transfer_complate)
    hal_i2c_s_dma_write                      0x000197d5   Thumb Code    52  hal_i2c_slave.o(i.hal_i2c_s_dma_write)
    hal_i2c_s_init                           0x00019811   Thumb Code    92  hal_i2c_slave.o(i.hal_i2c_s_init)
    hal_i2c_s_nonblocking_read               0x0001987d   Thumb Code    14  hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read)
    hal_i2c_s_set_transfer                   0x00019891   Thumb Code     6  hal_i2c_slave.o(i.hal_i2c_s_set_transfer)
    hal_internal_init_memc                   0x000199ed   Thumb Code    96  hal_internal_vsync.o(i.hal_internal_init_memc)
    hal_internal_sync_get_fb_setting         0x00019a9d   Thumb Code    12  hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting)
    hal_internal_sync_input_resolution_change 0x00019aad   Thumb Code   414  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    hal_internal_sync_set_fb_setting_manual  0x00019cf9   Thumb Code   372  hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual)
    hal_internal_vsync_deinit                0x00019e81   Thumb Code    24  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    hal_internal_vsync_get_rx_state          0x00019e9d   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state)
    hal_internal_vsync_get_sync_line         0x00019ea9   Thumb Code    24  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    hal_internal_vsync_get_tx_state          0x00019ec5   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    hal_internal_vsync_get_y2t4_use_sclu     0x00019ed1   Thumb Code    28  hal_internal_vsync.o(i.hal_internal_vsync_get_y2t4_use_sclu)
    hal_internal_vsync_init_rx               0x00019ef1   Thumb Code   166  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    hal_internal_vsync_init_tx               0x00019fad   Thumb Code   160  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    hal_internal_vsync_set_auto_hw_filter    0x0001a051   Thumb Code   222  hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter)
    hal_internal_vsync_set_rx_state          0x0001a16d   Thumb Code    20  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    hal_internal_vsync_set_sync_line         0x0001a185   Thumb Code    26  hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line)
    hal_internal_vsync_set_tear_mode         0x0001a1a5   Thumb Code    64  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    hal_internal_vsync_set_tx_state          0x0001a1ed   Thumb Code    58  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    hal_spi_m_clear_rxfifo                   0x0001a6a1   Thumb Code    14  hal_spi_master.o(i.hal_spi_m_clear_rxfifo)
    hal_swire_open                           0x0001a6af   Thumb Code    22  hal_swire.o(i.hal_swire_open)
    hal_system_enable_systick                0x0001a6c5   Thumb Code     8  hal_system.o(i.hal_system_enable_systick)
    hal_system_init                          0x0001a6cd   Thumb Code   104  hal_system.o(i.hal_system_init)
    hal_system_init_console                  0x0001a755   Thumb Code    28  hal_system.o(i.hal_system_init_console)
    hal_system_set_pvd                       0x0001a771   Thumb Code     8  hal_system.o(i.hal_system_set_pvd)
    hal_system_set_vcc                       0x0001a779   Thumb Code     8  hal_system.o(i.hal_system_set_vcc)
    hal_timer_init                           0x0001a781   Thumb Code    26  hal_timer.o(i.hal_timer_init)
    hal_timer_start                          0x0001a79d   Thumb Code    66  hal_timer.o(i.hal_timer_start)
    hal_timer_stop                           0x0001a7e5   Thumb Code    40  hal_timer.o(i.hal_timer_stop)
    hal_uart_init                            0x0001a80d   Thumb Code   126  hal_uart.o(i.hal_uart_init)
    hal_uart_transmit_blocking               0x0001a899   Thumb Code    12  hal_uart.o(i.hal_uart_transmit_blocking)
    handle_init                              0x0001a8a9   Thumb Code   136  irq_redirect .o(i.handle_init)
    main                                     0x0001aad1   Thumb Code    10  main.o(i.main)
    tp_heartbeat_exec                        0x0001b44d   Thumb Code    56  ap_demo.o(i.tp_heartbeat_exec)
    phone_data_21                            0x0001b828   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_55                            0x0001b829   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_85_1                          0x0001b82a   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_92_1                          0x0001b82b   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_F5_1                          0x0001b82c   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_F5_2                          0x0001b82d   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_F5_3                          0x0001b82e   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_F5_4                          0x0001b82f   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_30                            0x0001b830   Data           2  app_tp_for_custom_s8.o(.constdata)
    phone_data_52                            0x0001b832   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_data_92_3                          0x0001b835   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_data_A3                            0x0001b838   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_data_A4                            0x0001b83c   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_data_A5                            0x0001b840   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_data_AF                            0x0001b844   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_data_F1                            0x0001b848   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_data_22                            0x0001b84c   Data           5  app_tp_for_custom_s8.o(.constdata)
    phone_data_92_2                          0x0001b851   Data           6  app_tp_for_custom_s8.o(.constdata)
    phone_data_F6_1                          0x0001b857   Data           6  app_tp_for_custom_s8.o(.constdata)
    phone_data_F6_2                          0x0001b85d   Data           6  app_tp_for_custom_s8.o(.constdata)
    phone_data_F6_3                          0x0001b863   Data           6  app_tp_for_custom_s8.o(.constdata)
    phone_data_F6_4                          0x0001b869   Data           6  app_tp_for_custom_s8.o(.constdata)
    phone_data_60_1                          0x0001b86f   Data          16  app_tp_for_custom_s8.o(.constdata)
    phone_data_23                            0x0001b87f   Data          11  app_tp_for_custom_s8.o(.constdata)
    phone_data_85_2                          0x0001b88a   Data          28  app_tp_for_custom_s8.o(.constdata)
    phone_data_90                            0x0001b8a6   Data          10  app_tp_for_custom_s8.o(.constdata)
    phone_data_72_0                          0x0001b8b0   Data        1292  app_tp_for_custom_s8.o(.constdata)
    phone_data_72_5                          0x0001bdbc   Data        1292  app_tp_for_custom_s8.o(.constdata)
    phone_data_72_13                         0x0001c2c8   Data        1292  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_01                         0x0001c7d4   Data         654  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_02                         0x0001ca62   Data         654  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_03                         0x0001ccf0   Data         654  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_06                         0x0001cf7e   Data         654  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_07                         0x0001d20c   Data         654  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_05                         0x0001d49a   Data         654  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_00                         0x0001d728   Data         288  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_FF                         0x0001d848   Data         288  app_tp_for_custom_s8.o(.constdata)
    sleep_on                                 0x0001d968   Data          16  app_tp_for_custom_s8.o(.constdata)
    Region$$Table$$Base                      0x0001de54   Number         0  anon$$obj.o(Region$$Table)
    Region$$Table$$Limit                     0x0001de84   Number         0  anon$$obj.o(Region$$Table)
    g_fun_handle                             0x00070100   Data         192  irq_redirect .o(.ARM.__AT_0x00070100)
    phone_86_flag                            0x000701d6   Data           1  ap_demo.o(.data)
    phone_A6_flag                            0x000701d7   Data           1  ap_demo.o(.data)
    phone_start_flag                         0x000701d8   Data           1  ap_demo.o(.data)
    phone_DisplayOFF_flag                    0x000701d9   Data           1  ap_demo.o(.data)
    ap_tear_flag                             0x000701de   Data           1  ap_demo.o(.data)
    g_enter_display_off                      0x000701df   Data           1  ap_demo.o(.data)
    panel_mode                               0x000701e1   Data           1  ap_demo.o(.data)
    phone_DisplayOFF_count                   0x000701e4   Data           2  ap_demo.o(.data)
    value_reg_b1                             0x000701e6   Data           2  ap_demo.o(.data)
    value_reg_b1_bak                         0x000701e8   Data           2  ap_demo.o(.data)
    value_reg51                              0x000701ea   Data           2  ap_demo.o(.data)
    value_reg51_bak                          0x000701ec   Data           2  ap_demo.o(.data)
    panel_r                                  0x000701ee   Data           2  ap_demo.o(.data)
    panel_g                                  0x000701f0   Data           2  ap_demo.o(.data)
    panel_b                                  0x000701f2   Data           2  ap_demo.o(.data)
    s_heartbeat                              0x000701fc   Data           4  ap_demo.o(.data)
    value_reg_ca                             0x00070200   Data           4  ap_demo.o(.data)
    panel_init_code                          0x00070208   Data        9953  ap_demo.o(.data)
    phone_data_E4                            0x000728ea   Data           1  app_tp_for_custom_s8.o(.data)
    tp_flag                                  0x000728eb   Data           1  app_tp_for_custom_s8.o(.data)
    g_phone_output_int_pad                   0x000728ec   Data           1  app_tp_for_custom_s8.o(.data)
    tp_sleep_in                              0x000728ed   Data           1  app_tp_for_custom_s8.o(.data)
    tp_sleep_count                           0x000728ee   Data           1  app_tp_for_custom_s8.o(.data)
    sleep_double_EN                          0x000728ef   Data           1  app_tp_for_custom_s8.o(.data)
    Flag_EA_EN                               0x000728f0   Data           1  app_tp_for_custom_s8.o(.data)
    Flag_touch_count                         0x000728f1   Data           1  app_tp_for_custom_s8.o(.data)
    touchnum_bak                             0x000728f2   Data           1  app_tp_for_custom_s8.o(.data)
    Flag_blacklight_EN                       0x000728f3   Data           1  app_tp_for_custom_s8.o(.data)
    phone_data_B1                            0x000728fc   Data           2  app_tp_for_custom_s8.o(.data)
    phone_reg_coord_back                     0x00072906   Data         200  app_tp_for_custom_s8.o(.data)
    g_screen_input_rst_pad                   0x000729ce   Data           1  app_tp_for_custom_s8.o(.data)
    g_screen_input_int_pad                   0x000729cf   Data           1  app_tp_for_custom_s8.o(.data)
    screen_data_write_1                      0x000729d0   Data           1  app_tp_for_custom_s8.o(.data)
    screen_data_write_2                      0x000729d1   Data           3  app_tp_for_custom_s8.o(.data)
    screen_data_write_3                      0x000729d4   Data           5  app_tp_for_custom_s8.o(.data)
    screen_reg_int_data                      0x000729dc   Data          48  app_tp_for_custom_s8.o(.data)
    s_screen_init_complate                   0x00072a10   Data           1  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data1               0x00072a14   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data3               0x00072a17   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data4               0x00072a1a   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_TP_Tuning_data1                 0x00072a1d   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_TP_Tuning_data2                 0x00072a20   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_TP_Tuning_data3                 0x00072a23   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_TP_Tuning_data6                 0x00072a26   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_TP_Tuning_data7                 0x00072a29   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_TP_Tuning_data8                 0x00072a2c   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_TP_Tuning_data4                 0x00072a2f   Data           4  app_tp_transfer.o(.data)
    MI10_PRO_TP_Tuning_data5                 0x00072a33   Data           4  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data2               0x00072a37   Data           6  app_tp_transfer.o(.data)
    g_fls_w_cmd                              0x00072a68   Data           1  norflash.o(.data)
    g_fls_r_cmd                              0x00072a69   Data           1  norflash.o(.data)
    g_fls_write_en_status                    0x00072a6a   Data           1  norflash.o(.data)
    isFlsTransferEnd                         0x00072a6b   Data           1  norflash.o(.data)
    isFlsFifoReq                             0x00072a6c   Data           1  norflash.o(.data)
    isNandWriteCompleted                     0x00072a6d   Data           1  norflash.o(.data)
    isNandReadCompleted                      0x00072a6e   Data           1  norflash.o(.data)
    g_fls_error_info                         0x00072a74   Data           6  norflash.o(.data)
    g_systick_cb_func                        0x00072a80   Data           4  drv_common.o(.data)
    g_system_clock                           0x00072a84   Data           4  drv_common.o(.data)
    tx_byte_num                              0x00072a9c   Data           4  drv_i2c_slave.o(.data)
    g_scld_filter_h                          0x00072aa0   Data         256  drv_param_init.o(.data)
    g_scld_filter_v                          0x00072ba0   Data         256  drv_param_init.o(.data)
    g_scld_720_filter_h                      0x00072ca0   Data         256  drv_param_init.o(.data)
    g_scld_720_filter_v                      0x00072da0   Data         256  drv_param_init.o(.data)
    g_sclu_filter_h                          0x00072ea0   Data         256  drv_param_init.o(.data)
    g_sclu_filter_v                          0x00072fa0   Data         256  drv_param_init.o(.data)
    g_pq_setting                             0x000730a0   Data          40  drv_param_init.o(.data)
    g_ccm_setting                            0x000730c8   Data          36  drv_param_init.o(.data)
    __stdout                                 0x00073178   Data           4  stdout.o(.data)
    tp_scan_data                             0x0007330c   Data          12  app_tp_transfer.o(.bss)
    string                                   0x00073410   Data         256  tau_log.o(.bss)
    hal_dmahandle                            0x00073510   Data          12  hal_uart.o(.bss)
    hal_uarthandle_dma                       0x0007351c   Data          32  hal_uart.o(.bss)
    hal_uart_handle_global                   0x0007353c   Data          16  hal_uart.o(.bss)
    g_packet_fifo                            0x000735bc   Data        2764  dcs_packet_fifo.o(.bss)
    g_spis_ctrl_handle                       0x000749f0   Data          32  hal_spi_slave.o(.bss)
    __stack_limit                            0x00074a10   Data           0  startup_armcm0.o(STACK)
    __initial_sp                             0x00075a10   Data           0  startup_armcm0.o(STACK)



==============================================================================

Memory Map of the image

  Image Entry point : 0x000100c1

  Load Region LR_IROM2 (Base: 0x00010000, Size: 0x00010e30, Max: 0x00010000, ABSOLUTE, COMPRESSED[0x0000fdac])

    Execution Region ER_IROM2 (Exec base: 0x00010000, Load base: 0x00010000, Size: 0x0000de84, Max: 0x00010000, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00010000   0x00010000   0x000000c0   Data   RO          587    RESET               startup_armcm0.o
    0x000100c0   0x000100c0   0x00000000   Code   RO         2568  * .ARM.Collect$$$$00000000  mc_p.l(entry.o)
    0x000100c0   0x000100c0   0x00000004   Code   RO         2870    .ARM.Collect$$$$00000001  mc_p.l(entry2.o)
    0x000100c4   0x000100c4   0x00000004   Code   RO         2873    .ARM.Collect$$$$00000004  mc_p.l(entry5.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         2875    .ARM.Collect$$$$00000008  mc_p.l(entry7b.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         2877    .ARM.Collect$$$$0000000A  mc_p.l(entry8b.o)
    0x000100c8   0x000100c8   0x00000008   Code   RO         2878    .ARM.Collect$$$$0000000B  mc_p.l(entry9a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         2880    .ARM.Collect$$$$0000000D  mc_p.l(entry10a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         2882    .ARM.Collect$$$$0000000F  mc_p.l(entry11a.o)
    0x000100d0   0x000100d0   0x00000004   Code   RO         2871    .ARM.Collect$$$$00002712  mc_p.l(entry2.o)
    0x000100d4   0x000100d4   0x00000078   Code   RO          588    .text               startup_armcm0.o
    0x0001014c   0x0001014c   0x0000002c   Code   RO         2571    .text               mc_p.l(uidiv.o)
    0x00010178   0x00010178   0x00000028   Code   RO         2573    .text               mc_p.l(idiv.o)
    0x000101a0   0x000101a0   0x00000024   Code   RO         2575    .text               mc_p.l(memcpya.o)
    0x000101c4   0x000101c4   0x00000024   Code   RO         2577    .text               mc_p.l(memseta.o)
    0x000101e8   0x000101e8   0x000000b2   Code   RO         2842    .text               mf_p.l(fadd.o)
    0x0001029a   0x0001029a   0x0000007a   Code   RO         2844    .text               mf_p.l(fmul.o)
    0x00010314   0x00010314   0x0000007c   Code   RO         2846    .text               mf_p.l(fdiv.o)
    0x00010390   0x00010390   0x00000018   Code   RO         2848    .text               mf_p.l(fscalb.o)
    0x000103a8   0x000103a8   0x00000164   Code   RO         2850    .text               mf_p.l(dadd.o)
    0x0001050c   0x0001050c   0x00000016   Code   RO         2852    .text               mf_p.l(fflti.o)
    0x00010522   0x00010522   0x0000000e   Code   RO         2854    .text               mf_p.l(ffltui.o)
    0x00010530   0x00010530   0x0000001c   Code   RO         2856    .text               mf_p.l(dfltui.o)
    0x0001054c   0x0001054c   0x00000032   Code   RO         2858    .text               mf_p.l(ffixi.o)
    0x0001057e   0x0001057e   0x00000028   Code   RO         2860    .text               mf_p.l(ffixui.o)
    0x000105a6   0x000105a6   0x00000002   PAD
    0x000105a8   0x000105a8   0x00000048   Code   RO         2862    .text               mf_p.l(dfixi.o)
    0x000105f0   0x000105f0   0x0000003c   Code   RO         2864    .text               mf_p.l(dfixui.o)
    0x0001062c   0x0001062c   0x00000028   Code   RO         2866    .text               mf_p.l(f2d.o)
    0x00010654   0x00010654   0x00000014   Code   RO         2868    .text               mf_p.l(cfrcmple.o)
    0x00010668   0x00010668   0x00000060   Code   RO         2885    .text               mc_p.l(uldiv.o)
    0x000106c8   0x000106c8   0x00000020   Code   RO         2887    .text               mc_p.l(llshl.o)
    0x000106e8   0x000106e8   0x00000022   Code   RO         2889    .text               mc_p.l(llushr.o)
    0x0001070a   0x0001070a   0x00000026   Code   RO         2891    .text               mc_p.l(llsshr.o)
    0x00010730   0x00010730   0x00000000   Code   RO         2893    .text               mc_p.l(iusefp.o)
    0x00010730   0x00010730   0x00000082   Code   RO         2894    .text               mf_p.l(fepilogue.o)
    0x000107b2   0x000107b2   0x000000be   Code   RO         2896    .text               mf_p.l(depilogue.o)
    0x00010870   0x00010870   0x000000d0   Code   RO         2900    .text               mf_p.l(dmul.o)
    0x00010940   0x00010940   0x000000f0   Code   RO         2902    .text               mf_p.l(ddiv.o)
    0x00010a30   0x00010a30   0x00000040   Code   RO         2904    .text               mf_p.l(dfixul.o)
    0x00010a70   0x00010a70   0x00000028   Code   RO         2906    .text               mf_p.l(cdrcmple.o)
    0x00010a98   0x00010a98   0x00000024   Code   RO         2908    .text               mc_p.l(init.o)
    0x00010abc   0x00010abc   0x00000056   Code   RO         2918    .text               mc_p.l(__dczerorl2.o)
    0x00010b12   0x00010b12   0x00000002   PAD
    0x00010b14   0x00010b14   0x00000018   Code   RO         2218    i.ADC_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010b2c   0x00010b2c   0x0000001c   Code   RO         2219    i.AP_NRESET_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010b48   0x00010b48   0x00000014   Code   RO         2220    i.DMA_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010b5c   0x00010b5c   0x0000001c   Code   RO         2221    i.EXTI_INT0_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010b78   0x00010b78   0x0000001c   Code   RO         2222    i.EXTI_INT1_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010b94   0x00010b94   0x0000001c   Code   RO         2223    i.EXTI_INT2_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010bb0   0x00010bb0   0x0000001c   Code   RO         2224    i.EXTI_INT3_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010bcc   0x00010bcc   0x0000001c   Code   RO         2225    i.EXTI_INT4_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010be8   0x00010be8   0x0000001c   Code   RO         2226    i.EXTI_INT5_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010c04   0x00010c04   0x0000001c   Code   RO         2227    i.EXTI_INT6_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010c20   0x00010c20   0x0000001c   Code   RO         2228    i.EXTI_INT7_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010c3c   0x00010c3c   0x00000014   Code   RO         2229    i.FLSCTRL_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010c50   0x00010c50   0x00000074   Code   RO           99    i.Gpio_swire_output  ap_demo.o
    0x00010cc4   0x00010cc4   0x00000014   Code   RO         2230    i.HardFault_Handler  CVWL518.lib(irq_redirect .o)
    0x00010cd8   0x00010cd8   0x00000018   Code   RO         2231    i.I2C0_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010cf0   0x00010cf0   0x00000018   Code   RO         2232    i.I2C1_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010d08   0x00010d08   0x00000018   Code   RO         2233    i.LCDC_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010d20   0x00010d20   0x00000028   Code   RO          978    i.LOG_printf        CVWL518.lib(tau_log.o)
    0x00010d48   0x00010d48   0x00000018   Code   RO         2234    i.MEMC_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010d60   0x00010d60   0x00000018   Code   RO         2235    i.MIPI_RX_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010d78   0x00010d78   0x00000018   Code   RO         2236    i.MIPI_TX_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010d90   0x00010d90   0x0000001c   Code   RO         2237    i.PWMDET_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010dac   0x00010dac   0x00000124   Code   RO          376    i.S20_Start_init    app_tp_transfer.o
    0x00010ed0   0x00010ed0   0x0000001c   Code   RO         2238    i.SPIM_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010eec   0x00010eec   0x0000001c   Code   RO         2239    i.SPIS_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010f08   0x00010f08   0x0000001c   Code   RO         2240    i.SWIRE_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010f24   0x00010f24   0x00000018   Code   RO         2241    i.SysTick_Handler   CVWL518.lib(irq_redirect .o)
    0x00010f3c   0x00010f3c   0x00000018   Code   RO         2242    i.TIMER0_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010f54   0x00010f54   0x00000018   Code   RO         2243    i.TIMER1_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010f6c   0x00010f6c   0x00000018   Code   RO         2244    i.TIMER2_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010f84   0x00010f84   0x00000018   Code   RO         2245    i.TIMER3_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010f9c   0x00010f9c   0x00000002   Code   RO         2430    i.UART_DisableDma   CVWL518.lib(drv_uart.o)
    0x00010f9e   0x00010f9e   0x00000004   Code   RO         2436    i.UART_GetInstance  CVWL518.lib(drv_uart.o)
    0x00010fa2   0x00010fa2   0x00000002   PAD
    0x00010fa4   0x00010fa4   0x0000001c   Code   RO         2442    i.UART_IRQ_Handle   CVWL518.lib(drv_uart.o)
    0x00010fc0   0x00010fc0   0x00000018   Code   RO         2246    i.UART_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00010fd8   0x00010fd8   0x00000024   Code   RO         2445    i.UART_ResetRxFIFO  CVWL518.lib(drv_uart.o)
    0x00010ffc   0x00010ffc   0x00000002   Code   RO         2913    i.__scatterload_null  mc_p.l(handlers.o)
    0x00010ffe   0x00010ffe   0x00000001   Data   RO          305    .constdata          app_tp_for_custom_s8.o
    0x00010fff   0x00010fff   0x00000001   PAD
    0x00011000   0x00011000   0x00000014   Data   RO         1101    .ARM.__at_0x11000   CVWL518.lib(drv_common.o)
    0x00011014   0x00011014   0x00000048   Code   RO         2448    i.UART_SetBaudRate  CVWL518.lib(drv_uart.o)
    0x0001105c   0x0001105c   0x0000001a   Code   RO         2449    i.UART_SwitchSCLK   CVWL518.lib(drv_uart.o)
    0x00011076   0x00011076   0x00000134   Code   RO         2451    i.UART_TransferHandleIRQ  CVWL518.lib(drv_uart.o)
    0x000111aa   0x000111aa   0x0000001a   Code   RO         2453    i.UART_WriteBlocking  CVWL518.lib(drv_uart.o)
    0x000111c4   0x000111c4   0x000000bc   Code   RO         2454    i.UART_init         CVWL518.lib(drv_uart.o)
    0x00011280   0x00011280   0x00000018   Code   RO         2247    i.VIDC_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x00011298   0x00011298   0x00000018   Code   RO         2248    i.VPRE_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x000112b0   0x000112b0   0x00000018   Code   RO         2249    i.WDG_IRQn_Handler  CVWL518.lib(irq_redirect .o)
    0x000112c8   0x000112c8   0x00000020   Code   RO         2814    i.__0printf         mc_p.l(printfa.o)
    0x000112e8   0x000112e8   0x00000024   Code   RO         2820    i.__0vsprintf       mc_p.l(printfa.o)
    0x0001130c   0x0001130c   0x0000002e   Code   RO         2898    i.__ARM_clz         mf_p.l(depilogue.o)
    0x0001133a   0x0001133a   0x0000001a   Code   RO          244    i.__ARM_common_switch8  ap_demo.o
    0x00011354   0x00011354   0x00000018   Code   RO         1414    i.__NVIC_ClearPendingIRQ  CVWL518.lib(drv_i2c_master.o)
    0x0001136c   0x0001136c   0x00000018   Code   RO         1447    i.__NVIC_ClearPendingIRQ  CVWL518.lib(drv_i2c_slave.o)
    0x00011384   0x00011384   0x00000044   Code   RO         2318    i.__NVIC_SetPriority  CVWL518.lib(hal_spi_slave.o)
    0x000113c8   0x000113c8   0x0000000e   Code   RO         2912    i.__scatterload_copy  mc_p.l(handlers.o)
    0x000113d6   0x000113d6   0x0000000e   Code   RO         2914    i.__scatterload_zeroinit  mc_p.l(handlers.o)
    0x000113e4   0x000113e4   0x00000174   Code   RO         2821    i._fp_digits        mc_p.l(printfa.o)
    0x00011558   0x00011558   0x000006ec   Code   RO         2822    i._printf_core      mc_p.l(printfa.o)
    0x00011c44   0x00011c44   0x00000020   Code   RO         2823    i._printf_post_padding  mc_p.l(printfa.o)
    0x00011c64   0x00011c64   0x0000002c   Code   RO         2824    i._printf_pre_padding  mc_p.l(printfa.o)
    0x00011c90   0x00011c90   0x0000000a   Code   RO         2826    i._sputc            mc_p.l(printfa.o)
    0x00011c9a   0x00011c9a   0x00000002   PAD
    0x00011c9c   0x00011c9c   0x00001394   Code   RO          100    i.ap_dcs_read       ap_demo.o
    0x00013030   0x00013030   0x00000174   Code   RO          101    i.ap_demo           ap_demo.o
    0x000131a4   0x000131a4   0x0000002c   Code   RO          102    i.ap_get_reg_ca     ap_demo.o
    0x000131d0   0x000131d0   0x000000b0   Code   RO          103    i.ap_get_reg_df     ap_demo.o
    0x00013280   0x00013280   0x0000005c   Code   RO          104    i.ap_reset_cb       ap_demo.o
    0x000132dc   0x000132dc   0x00000360   Code   RO          105    i.ap_set_backlight  ap_demo.o
    0x0001363c   0x0001363c   0x00000058   Code   RO          106    i.ap_set_display_off  ap_demo.o
    0x00013694   0x00013694   0x00000044   Code   RO          107    i.ap_set_display_on  ap_demo.o
    0x000136d8   0x000136d8   0x00000060   Code   RO          108    i.ap_set_enter_sleep_mode  ap_demo.o
    0x00013738   0x00013738   0x00000048   Code   RO          109    i.ap_set_exit_sleep_mode  ap_demo.o
    0x00013780   0x00013780   0x0000001c   Code   RO          110    i.ap_set_tp_calibration_04  ap_demo.o
    0x0001379c   0x0001379c   0x000000b0   Code   RO          377    i.ap_tp_calibration  app_tp_transfer.o
    0x0001384c   0x0001384c   0x0000001c   Code   RO          378    i.ap_tp_scan_point_init  app_tp_transfer.o
    0x00013868   0x00013868   0x0000009c   Code   RO          379    i.ap_tp_scan_point_record_event  app_tp_transfer.o
    0x00013904   0x00013904   0x00000050   Code   RO          380    i.ap_tp_scan_point_record_event_exec  app_tp_transfer.o
    0x00013954   0x00013954   0x00000034   Code   RO          381    i.ap_tp_simulate_finger_release_event  app_tp_transfer.o
    0x00013988   0x00013988   0x00000040   Code   RO          382    i.ap_tp_system_softReset  app_tp_transfer.o
    0x000139c8   0x000139c8   0x00000024   Code   RO         1338    i.app_AP_NRESET_IRQn_Handler  CVWL518.lib(drv_gpio.o)
    0x000139ec   0x000139ec   0x0000001c   Code   RO         1339    i.app_EXTI_INT0_IRQn_Handler  CVWL518.lib(drv_gpio.o)
    0x00013a08   0x00013a08   0x0000001c   Code   RO         1340    i.app_EXTI_INT1_IRQn_Handler  CVWL518.lib(drv_gpio.o)
    0x00013a24   0x00013a24   0x0000001c   Code   RO         1341    i.app_EXTI_INT2_IRQn_Handler  CVWL518.lib(drv_gpio.o)
    0x00013a40   0x00013a40   0x0000001c   Code   RO         1342    i.app_EXTI_INT3_IRQn_Handler  CVWL518.lib(drv_gpio.o)
    0x00013a5c   0x00013a5c   0x0000001c   Code   RO         1343    i.app_EXTI_INT4_IRQn_Handler  CVWL518.lib(drv_gpio.o)
    0x00013a78   0x00013a78   0x0000001c   Code   RO         1344    i.app_EXTI_INT5_IRQn_Handler  CVWL518.lib(drv_gpio.o)
    0x00013a94   0x00013a94   0x0000001c   Code   RO         1345    i.app_EXTI_INT6_IRQn_Handler  CVWL518.lib(drv_gpio.o)
    0x00013ab0   0x00013ab0   0x0000001c   Code   RO         1346    i.app_EXTI_INT7_IRQn_Handler  CVWL518.lib(drv_gpio.o)
    0x00013acc   0x00013acc   0x00000048   Code   RO         1092    i.app_HardFault_Handler  CVWL518.lib(drv_common.o)
    0x00013b14   0x00013b14   0x00000010   Code   RO         1448    i.app_I2C0_IRQn_Handler  CVWL518.lib(drv_i2c_slave.o)
    0x00013b24   0x00013b24   0x00000010   Code   RO         1415    i.app_I2C1_IRQn_Handler  CVWL518.lib(drv_i2c_master.o)
    0x00013b34   0x00013b34   0x000000e0   Code   RO         1687    i.app_LCDC_IRQn_Handler  CVWL518.lib(hal_internal_vsync.o)
    0x00013c14   0x00013c14   0x00000060   Code   RO         1990    i.app_MEMC_IRQn_Handler  CVWL518.lib(drv_memc.o)
    0x00013c74   0x00013c74   0x00000298   Code   RO         1760    i.app_MIPI_RX_IRQn_Handler  CVWL518.lib(drv_dsi_rx.o)
    0x00013f0c   0x00013f0c   0x000000a0   Code   RO         1814    i.app_MIPI_TX_IRQn_Handler  CVWL518.lib(drv_dsi_tx.o)
    0x00013fac   0x00013fac   0x00000048   Code   RO         2388    i.app_PWMDET_IRQn_Handler  CVWL518.lib(drv_pwm.o)
    0x00013ff4   0x00013ff4   0x00000020   Code   RO         1562    i.app_SPIM_IRQn_Handler  CVWL518.lib(drv_spi_master.o)
    0x00014014   0x00014014   0x00000200   Code   RO         2319    i.app_SPIS_IRQn_Handler  CVWL518.lib(hal_spi_slave.o)
    0x00014214   0x00014214   0x00000020   Code   RO         1591    i.app_SWIRE_IRQn_Handler  CVWL518.lib(drv_swire.o)
    0x00014234   0x00014234   0x00000018   Code   RO         1093    i.app_SysTick_Handler  CVWL518.lib(drv_common.o)
    0x0001424c   0x0001424c   0x0000000a   Code   RO         1641    i.app_TIMER0_IRQn_Handler  CVWL518.lib(drv_timer.o)
    0x00014256   0x00014256   0x0000000a   Code   RO         1642    i.app_TIMER1_IRQn_Handler  CVWL518.lib(drv_timer.o)
    0x00014260   0x00014260   0x0000000a   Code   RO         1643    i.app_TIMER2_IRQn_Handler  CVWL518.lib(drv_timer.o)
    0x0001426a   0x0001426a   0x0000000a   Code   RO         1644    i.app_TIMER3_IRQn_Handler  CVWL518.lib(drv_timer.o)
    0x00014274   0x00014274   0x00000008   Code   RO         2455    i.app_UART_IRQn_Handler  CVWL518.lib(drv_uart.o)
    0x0001427c   0x0001427c   0x000000e4   Code   RO         1688    i.app_VIDC_IRQn_Handler  CVWL518.lib(hal_internal_vsync.o)
    0x00014360   0x00014360   0x00000284   Code   RO         1689    i.app_VPRE_IRQn_Handler  CVWL518.lib(hal_internal_vsync.o)
    0x000145e4   0x000145e4   0x00000038   Code   RO         2514    i.app_WDG_IRQn_Handler  CVWL518.lib(drv_wdg.o)
    0x0001461c   0x0001461c   0x00000008   Code   RO         1202    i.app_dma_irq_handler  CVWL518.lib(drv_dma.o)
    0x00014624   0x00014624   0x00000030   Code   RO          989    i.app_fls_ctrl_Handler  CVWL518.lib(norflash.o)
    0x00014654   0x00014654   0x00000024   Code   RO          383    i.app_tp_I2C_init   app_tp_transfer.o
    0x00014678   0x00014678   0x0000005c   Code   RO          111    i.app_tp_calibration_exec  ap_demo.o
    0x000146d4   0x000146d4   0x0000000a   Code   RO          384    i.app_tp_i2cs_callback  app_tp_transfer.o
    0x000146de   0x000146de   0x00000002   PAD
    0x000146e0   0x000146e0   0x00000048   Code   RO          385    i.app_tp_init       app_tp_transfer.o
    0x00014728   0x00014728   0x00000020   Code   RO          386    i.app_tp_m_read     app_tp_transfer.o
    0x00014748   0x00014748   0x00000008   Code   RO          387    i.app_tp_m_transfer_complate  app_tp_transfer.o
    0x00014750   0x00014750   0x00000008   Code   RO          388    i.app_tp_m_write    app_tp_transfer.o
    0x00014758   0x00014758   0x00000410   Code   RO          288    i.app_tp_phone_analysis_data  app_tp_for_custom_s8.o
    0x00014b68   0x00014b68   0x0000000c   Code   RO          389    i.app_tp_phone_clear_reset_on  app_tp_transfer.o
    0x00014b74   0x00014b74   0x00000008   Code   RO          391    i.app_tp_s_read     app_tp_transfer.o
    0x00014b7c   0x00014b7c   0x00000008   Code   RO          393    i.app_tp_s_write    app_tp_transfer.o
    0x00014b84   0x00014b84   0x000002cc   Code   RO          290    i.app_tp_screen_analysis_int  app_tp_for_custom_s8.o
    0x00014e50   0x00014e50   0x00000030   Code   RO          394    i.app_tp_screen_init  app_tp_transfer.o
    0x00014e80   0x00014e80   0x0000000c   Code   RO          395    i.app_tp_screen_int_callback  app_tp_transfer.o
    0x00014e8c   0x00014e8c   0x00000038   Code   RO          396    i.app_tp_screen_int_init  app_tp_transfer.o
    0x00014ec4   0x00014ec4   0x00000004   Code   RO          397    i.app_tp_screen_int_lvl_low  app_tp_transfer.o
    0x00014ec8   0x00014ec8   0x00000030   Code   RO          398    i.app_tp_transfer_phone  app_tp_transfer.o
    0x00014ef8   0x00014ef8   0x00000040   Code   RO          399    i.app_tp_transfer_screen_const  app_tp_transfer.o
    0x00014f38   0x00014f38   0x000001e0   Code   RO          400    i.app_tp_transfer_screen_int  app_tp_transfer.o
    0x00015118   0x00015118   0x00000018   Code   RO          401    i.app_tp_transfer_screen_start  app_tp_transfer.o
    0x00015130   0x00015130   0x00000036   Code   RO          112    i.blue_change_ccm   ap_demo.o
    0x00015166   0x00015166   0x00000002   PAD
    0x00015168   0x00015168   0x0000001c   Code   RO          567    i.board_Init        board.o
    0x00015184   0x00015184   0x000001ec   Code   RO         1690    i.calc_framebuffer_setting  CVWL518.lib(hal_internal_vsync.o)
    0x00015370   0x00015370   0x000000c8   Code   RO         2565    i.ceil              m_ps.l(ceil.o)
    0x00015438   0x00015438   0x0000002c   Code   RO         1691    i.check_mipi_rx_tx_video_info  CVWL518.lib(hal_internal_vsync.o)
    0x00015464   0x00015464   0x0000002c   Code   RO         1692    i.check_pkt_buf_rev  CVWL518.lib(hal_internal_vsync.o)
    0x00015490   0x00015490   0x00000058   Code   RO         1674    i.dcs_packet_fifo_alloc  CVWL518.lib(dcs_packet_fifo.o)
    0x000154e8   0x000154e8   0x00000018   Code   RO         1675    i.dcs_packet_fifo_init  CVWL518.lib(dcs_packet_fifo.o)
    0x00015500   0x00015500   0x00000044   Code   RO         1676    i.dcs_packet_free_fifo_header  CVWL518.lib(dcs_packet_fifo.o)
    0x00015544   0x00015544   0x00000024   Code   RO         1677    i.dcs_packet_get_fifo_header  CVWL518.lib(dcs_packet_fifo.o)
    0x00015568   0x00015568   0x0000001c   Code   RO         1693    i.dcs_sw_filter     CVWL518.lib(hal_internal_vsync.o)
    0x00015584   0x00015584   0x00000018   Code   RO          970    i.delayMs           CVWL518.lib(tau_delay.o)
    0x0001559c   0x0001559c   0x00000022   Code   RO          971    i.delayUs           CVWL518.lib(tau_delay.o)
    0x000155be   0x000155be   0x00000002   PAD
    0x000155c0   0x000155c0   0x00000094   Code   RO          113    i.disable_mipi_timer_cb  ap_demo.o
    0x00015654   0x00015654   0x00000038   Code   RO         1610    i.drv_ap_rst_trig_edge_detect  CVWL518.lib(drv_sys_cfg.o)
    0x0001568c   0x0001568c   0x0000000c   Code   RO         2289    i.drv_chip_info_get_version  CVWL518.lib(drv_chip_info.o)
    0x00015698   0x00015698   0x000000b0   Code   RO         2290    i.drv_chip_info_init  CVWL518.lib(drv_chip_info.o)
    0x00015748   0x00015748   0x0000005c   Code   RO         2291    i.drv_chip_rx_info_check  CVWL518.lib(drv_chip_info.o)
    0x000157a4   0x000157a4   0x00000014   Code   RO         2292    i.drv_chip_rx_init_done  CVWL518.lib(drv_chip_info.o)
    0x000157b8   0x000157b8   0x00000058   Code   RO         1095    i.drv_common_enable_systick  CVWL518.lib(drv_common.o)
    0x00015810   0x00015810   0x00000030   Code   RO         1099    i.drv_common_system_init  CVWL518.lib(drv_common.o)
    0x00015840   0x00015840   0x00000010   Code   RO         1121    i.drv_crgu_config_reset_modules  CVWL518.lib(drv_crgu.o)
    0x00015850   0x00015850   0x00000014   Code   RO         1133    i.drv_crgu_set_ahb_pre_div  CVWL518.lib(drv_crgu.o)
    0x00015864   0x00015864   0x00000014   Code   RO         1134    i.drv_crgu_set_ahb_src  CVWL518.lib(drv_crgu.o)
    0x00015878   0x00015878   0x00000020   Code   RO         1135    i.drv_crgu_set_clock  CVWL518.lib(drv_crgu.o)
    0x00015898   0x00015898   0x00000014   Code   RO         1136    i.drv_crgu_set_dpi_mux_src  CVWL518.lib(drv_crgu.o)
    0x000158ac   0x000158ac   0x00000018   Code   RO         1137    i.drv_crgu_set_dpi_pre_div  CVWL518.lib(drv_crgu.o)
    0x000158c4   0x000158c4   0x00000014   Code   RO         1138    i.drv_crgu_set_dpi_pre_src  CVWL518.lib(drv_crgu.o)
    0x000158d8   0x000158d8   0x00000014   Code   RO         1139    i.drv_crgu_set_dsc_core_div  CVWL518.lib(drv_crgu.o)
    0x000158ec   0x000158ec   0x00000014   Code   RO         1140    i.drv_crgu_set_dsco_src  CVWL518.lib(drv_crgu.o)
    0x00015900   0x00015900   0x00000014   Code   RO         1141    i.drv_crgu_set_dsco_src_div  CVWL518.lib(drv_crgu.o)
    0x00015914   0x00015914   0x00000014   Code   RO         1142    i.drv_crgu_set_fb_div  CVWL518.lib(drv_crgu.o)
    0x00015928   0x00015928   0x00000014   Code   RO         1143    i.drv_crgu_set_fb_src  CVWL518.lib(drv_crgu.o)
    0x0001593c   0x0001593c   0x00000014   Code   RO         1146    i.drv_crgu_set_lcdc_div  CVWL518.lib(drv_crgu.o)
    0x00015950   0x00015950   0x00000014   Code   RO         1147    i.drv_crgu_set_lcdc_src  CVWL518.lib(drv_crgu.o)
    0x00015964   0x00015964   0x00000014   Code   RO         1148    i.drv_crgu_set_mipi_cfg_src  CVWL518.lib(drv_crgu.o)
    0x00015978   0x00015978   0x00000018   Code   RO         1149    i.drv_crgu_set_mipi_ref_src  CVWL518.lib(drv_crgu.o)
    0x00015990   0x00015990   0x00000018   Code   RO         1152    i.drv_crgu_set_reset  CVWL518.lib(drv_crgu.o)
    0x000159a8   0x000159a8   0x00000014   Code   RO         1153    i.drv_crgu_set_rxbr_div  CVWL518.lib(drv_crgu.o)
    0x000159bc   0x000159bc   0x00000014   Code   RO         1154    i.drv_crgu_set_rxbr_src  CVWL518.lib(drv_crgu.o)
    0x000159d0   0x000159d0   0x00000014   Code   RO         1156    i.drv_crgu_set_vidc_src  CVWL518.lib(drv_crgu.o)
    0x000159e4   0x000159e4   0x0000001c   Code   RO         1206    i.drv_dma_clear_flag  CVWL518.lib(drv_dma.o)
    0x00015a00   0x00015a00   0x00000018   Code   RO         1207    i.drv_dma_create_handle  CVWL518.lib(drv_dma.o)
    0x00015a18   0x00015a18   0x00000018   Code   RO         1209    i.drv_dma_disenable_channel  CVWL518.lib(drv_dma.o)
    0x00015a30   0x00015a30   0x00000018   Code   RO         1211    i.drv_dma_enable_channel  CVWL518.lib(drv_dma.o)
    0x00015a48   0x00015a48   0x00000034   Code   RO         1212    i.drv_dma_enable_channel_interrupts  CVWL518.lib(drv_dma.o)
    0x00015a7c   0x00015a7c   0x00000030   Code   RO         1213    i.drv_dma_enable_cycle  CVWL518.lib(drv_dma.o)
    0x00015aac   0x00015aac   0x00000014   Code   RO         1214    i.drv_dma_get_channel_flag  CVWL518.lib(drv_dma.o)
    0x00015ac0   0x00015ac0   0x0000007c   Code   RO         1217    i.drv_dma_irq_handler  CVWL518.lib(drv_dma.o)
    0x00015b3c   0x00015b3c   0x00000018   Code   RO         1219    i.drv_dma_prepar_transfer  CVWL518.lib(drv_dma.o)
    0x00015b54   0x00015b54   0x0000001c   Code   RO         1221    i.drv_dma_set_burst  CVWL518.lib(drv_dma.o)
    0x00015b70   0x00015b70   0x00000006   Code   RO         1222    i.drv_dma_set_callback  CVWL518.lib(drv_dma.o)
    0x00015b76   0x00015b76   0x00000002   PAD
    0x00015b78   0x00015b78   0x00000044   Code   RO         1224    i.drv_dma_set_transfer  CVWL518.lib(drv_dma.o)
    0x00015bbc   0x00015bbc   0x00000036   Code   RO         2302    i.drv_dsc_dec_convert_pps_rc_parameter  CVWL518.lib(drv_dsc_dec.o)
    0x00015bf2   0x00015bf2   0x0000000c   Code   RO         2303    i.drv_dsc_dec_disable  CVWL518.lib(drv_dsc_dec.o)
    0x00015bfe   0x00015bfe   0x00000002   PAD
    0x00015c00   0x00015c00   0x000000b4   Code   RO         2304    i.drv_dsc_dec_enable  CVWL518.lib(drv_dsc_dec.o)
    0x00015cb4   0x00015cb4   0x0000000a   Code   RO         2305    i.drv_dsc_dec_get_nslc  CVWL518.lib(drv_dsc_dec.o)
    0x00015cbe   0x00015cbe   0x00000028   Code   RO         2307    i.drv_dsc_dec_set_u8_pps  CVWL518.lib(drv_dsc_dec.o)
    0x00015ce6   0x00015ce6   0x00000002   PAD
    0x00015ce8   0x00015ce8   0x00000104   Code   RO         1761    i.drv_dsi_rx_calc_ipi_tx_delay  CVWL518.lib(drv_dsi_rx.o)
    0x00015dec   0x00015dec   0x00000040   Code   RO         1762    i.drv_dsi_rx_enable_irq  CVWL518.lib(drv_dsi_rx.o)
    0x00015e2c   0x00015e2c   0x00000050   Code   RO         1763    i.drv_dsi_rx_get_color_bpp  CVWL518.lib(drv_dsi_rx.o)
    0x00015e7c   0x00015e7c   0x0000001c   Code   RO         1764    i.drv_dsi_rx_get_color_pcc  CVWL518.lib(drv_dsi_rx.o)
    0x00015e98   0x00015e98   0x00000008   Code   RO         1765    i.drv_dsi_rx_get_compression_en  CVWL518.lib(drv_dsi_rx.o)
    0x00015ea0   0x00015ea0   0x00000006   Code   RO         1766    i.drv_dsi_rx_get_max_ret_size  CVWL518.lib(drv_dsi_rx.o)
    0x00015ea6   0x00015ea6   0x0000000e   Code   RO         1770    i.drv_dsi_rx_power_up  CVWL518.lib(drv_dsi_rx.o)
    0x00015eb4   0x00015eb4   0x0000001c   Code   RO         1771    i.drv_dsi_rx_set_ctrl_cfg  CVWL518.lib(drv_dsi_rx.o)
    0x00015ed0   0x00015ed0   0x00000010   Code   RO         1772    i.drv_dsi_rx_set_ddi_cfg  CVWL518.lib(drv_dsi_rx.o)
    0x00015ee0   0x00015ee0   0x00000004   Code   RO         1774    i.drv_dsi_rx_set_inten  CVWL518.lib(drv_dsi_rx.o)
    0x00015ee4   0x00015ee4   0x00000010   Code   RO         1775    i.drv_dsi_rx_set_ipi_cfg  CVWL518.lib(drv_dsi_rx.o)
    0x00015ef4   0x00015ef4   0x00000026   Code   RO         1777    i.drv_dsi_rx_set_resp_cnt  CVWL518.lib(drv_dsi_rx.o)
    0x00015f1a   0x00015f1a   0x00000002   PAD
    0x00015f1c   0x00015f1c   0x00000090   Code   RO         1778    i.drv_dsi_rx_set_up_phy  CVWL518.lib(drv_dsi_rx.o)
    0x00015fac   0x00015fac   0x0000000e   Code   RO         1779    i.drv_dsi_rx_shut_down  CVWL518.lib(drv_dsi_rx.o)
    0x00015fba   0x00015fba   0x00000014   Code   RO         1816    i.drv_dsi_tx_command_header  CVWL518.lib(drv_dsi_tx.o)
    0x00015fce   0x00015fce   0x0000006c   Code   RO         1817    i.drv_dsi_tx_command_mode_cfg  CVWL518.lib(drv_dsi_tx.o)
    0x0001603a   0x0001603a   0x00000004   Code   RO         1818    i.drv_dsi_tx_command_put_payload  CVWL518.lib(drv_dsi_tx.o)
    0x0001603e   0x0001603e   0x00000018   Code   RO         1819    i.drv_dsi_tx_config_eotp  CVWL518.lib(drv_dsi_tx.o)
    0x00016056   0x00016056   0x00000008   Code   RO         1820    i.drv_dsi_tx_config_int  CVWL518.lib(drv_dsi_tx.o)
    0x0001605e   0x0001605e   0x00000008   Code   RO         1821    i.drv_dsi_tx_dpi_lpcmd_time  CVWL518.lib(drv_dsi_tx.o)
    0x00016066   0x00016066   0x0000000a   Code   RO         1822    i.drv_dsi_tx_dpi_mode  CVWL518.lib(drv_dsi_tx.o)
    0x00016070   0x00016070   0x00000024   Code   RO         1823    i.drv_dsi_tx_dpi_polarity  CVWL518.lib(drv_dsi_tx.o)
    0x00016094   0x00016094   0x00000004   Code   RO         1825    i.drv_dsi_tx_get_cmd_status  CVWL518.lib(drv_dsi_tx.o)
    0x00016098   0x00016098   0x00000004   Code   RO         1827    i.drv_dsi_tx_mode   CVWL518.lib(drv_dsi_tx.o)
    0x0001609c   0x0001609c   0x00000018   Code   RO         1828    i.drv_dsi_tx_phy_clock_lane_auto_lp  CVWL518.lib(drv_dsi_tx.o)
    0x000160b4   0x000160b4   0x0000001a   Code   RO         1829    i.drv_dsi_tx_phy_clock_lane_req_hs  CVWL518.lib(drv_dsi_tx.o)
    0x000160ce   0x000160ce   0x0000000c   Code   RO         1831    i.drv_dsi_tx_phy_lane_mode  CVWL518.lib(drv_dsi_tx.o)
    0x000160da   0x000160da   0x00000064   Code   RO         1835    i.drv_dsi_tx_phy_status_ready  CVWL518.lib(drv_dsi_tx.o)
    0x0001613e   0x0001613e   0x0000003e   Code   RO         1836    i.drv_dsi_tx_phy_status_stopstate  CVWL518.lib(drv_dsi_tx.o)
    0x0001617c   0x0001617c   0x000000e4   Code   RO         1838    i.drv_dsi_tx_phy_test_setup  CVWL518.lib(drv_dsi_tx.o)
    0x00016260   0x00016260   0x0000001e   Code   RO         1839    i.drv_dsi_tx_phy_time_cfg  CVWL518.lib(drv_dsi_tx.o)
    0x0001627e   0x0001627e   0x00000008   Code   RO         1843    i.drv_dsi_tx_powerup  CVWL518.lib(drv_dsi_tx.o)
    0x00016286   0x00016286   0x0000001c   Code   RO         1844    i.drv_dsi_tx_response_mode  CVWL518.lib(drv_dsi_tx.o)
    0x000162a2   0x000162a2   0x00000018   Code   RO         1847    i.drv_dsi_tx_set_bta_ack  CVWL518.lib(drv_dsi_tx.o)
    0x000162ba   0x000162ba   0x0000000c   Code   RO         1848    i.drv_dsi_tx_set_esc_div  CVWL518.lib(drv_dsi_tx.o)
    0x000162c6   0x000162c6   0x00000002   PAD
    0x000162c8   0x000162c8   0x00000034   Code   RO         1849    i.drv_dsi_tx_set_int  CVWL518.lib(drv_dsi_tx.o)
    0x000162fc   0x000162fc   0x00000010   Code   RO         1850    i.drv_dsi_tx_set_time_out_div  CVWL518.lib(drv_dsi_tx.o)
    0x0001630c   0x0001630c   0x00000008   Code   RO         1851    i.drv_dsi_tx_set_video_chunk  CVWL518.lib(drv_dsi_tx.o)
    0x00016314   0x00016314   0x00000022   Code   RO         1852    i.drv_dsi_tx_set_video_timing  CVWL518.lib(drv_dsi_tx.o)
    0x00016336   0x00016336   0x00000008   Code   RO         1854    i.drv_dsi_tx_shutdown  CVWL518.lib(drv_dsi_tx.o)
    0x0001633e   0x0001633e   0x00000026   Code   RO         1855    i.drv_dsi_tx_timeout_cfg  CVWL518.lib(drv_dsi_tx.o)
    0x00016364   0x00016364   0x000000aa   Code   RO         1858    i.drv_dsi_tx_video_mode_cfg  CVWL518.lib(drv_dsi_tx.o)
    0x0001640e   0x0001640e   0x00000016   Code   RO         1859    i.drv_dsi_tx_video_mode_disable_hact_cmd  CVWL518.lib(drv_dsi_tx.o)
    0x00016424   0x00016424   0x00000018   Code   RO         1860    i.drv_dsi_tx_video_mode_set_lp_cmd  CVWL518.lib(drv_dsi_tx.o)
    0x0001643c   0x0001643c   0x00000018   Code   RO         1347    i.drv_gpio_get_input_data  CVWL518.lib(drv_gpio.o)
    0x00016454   0x00016454   0x0000000c   Code   RO         1349    i.drv_gpio_register_ap_reset_callback  CVWL518.lib(drv_gpio.o)
    0x00016460   0x00016460   0x00000014   Code   RO         1350    i.drv_gpio_register_callback  CVWL518.lib(drv_gpio.o)
    0x00016474   0x00016474   0x00000044   Code   RO         1352    i.drv_gpio_set_int  CVWL518.lib(drv_gpio.o)
    0x000164b8   0x000164b8   0x00000020   Code   RO         1353    i.drv_gpio_set_ioe  CVWL518.lib(drv_gpio.o)
    0x000164d8   0x000164d8   0x00000010   Code   RO         1354    i.drv_gpio_set_mode0  CVWL518.lib(drv_gpio.o)
    0x000164e8   0x000164e8   0x00000010   Code   RO         1355    i.drv_gpio_set_mode1  CVWL518.lib(drv_gpio.o)
    0x000164f8   0x000164f8   0x00000010   Code   RO         1356    i.drv_gpio_set_mode2  CVWL518.lib(drv_gpio.o)
    0x00016508   0x00016508   0x00000010   Code   RO         1357    i.drv_gpio_set_mode3  CVWL518.lib(drv_gpio.o)
    0x00016518   0x00016518   0x00000020   Code   RO          786    i.drv_gpio_set_output_data  CVWL518.lib(hal_gpio.o)
    0x00016538   0x00016538   0x00000130   Code   RO         1358    i.drv_gpio_set_pull_state  CVWL518.lib(drv_gpio.o)
    0x00016668   0x00016668   0x00000060   Code   RO         1416    i.drv_i2c_clear_m_it_pending_bit  CVWL518.lib(drv_i2c_master.o)
    0x000166c8   0x000166c8   0x0000005c   Code   RO         1449    i.drv_i2c_clear_s_it_pending_bit  CVWL518.lib(drv_i2c_slave.o)
    0x00016724   0x00016724   0x00000034   Code   RO         1390    i.drv_i2c_dma_callback  CVWL518.lib(drv_i2c_dma.o)
    0x00016758   0x00016758   0x000000ac   Code   RO         1391    i.drv_i2c_dma_init  CVWL518.lib(drv_i2c_dma.o)
    0x00016804   0x00016804   0x0000001a   Code   RO         1392    i.drv_i2c_enable_rx_dma  CVWL518.lib(drv_i2c_dma.o)
    0x0001681e   0x0001681e   0x00000018   Code   RO         1393    i.drv_i2c_enable_tx_dma  CVWL518.lib(drv_i2c_dma.o)
    0x00016836   0x00016836   0x00000002   PAD
    0x00016838   0x00016838   0x00000038   Code   RO         1420    i.drv_i2c_m_enable_intr  CVWL518.lib(drv_i2c_master.o)
    0x00016870   0x00016870   0x0000000c   Code   RO         1423    i.drv_i2c_m_set_callback  CVWL518.lib(drv_i2c_master.o)
    0x0001687c   0x0001687c   0x0000008c   Code   RO         1427    i.drv_i2c_master_init  CVWL518.lib(drv_i2c_master.o)
    0x00016908   0x00016908   0x0000007c   Code   RO         1394    i.drv_i2c_master_read_dma  CVWL518.lib(drv_i2c_dma.o)
    0x00016984   0x00016984   0x00000040   Code   RO         1395    i.drv_i2c_master_write_dma  CVWL518.lib(drv_i2c_dma.o)
    0x000169c4   0x000169c4   0x0000002e   Code   RO         1396    i.drv_i2c_master_write_read_cmd  CVWL518.lib(drv_i2c_dma.o)
    0x000169f2   0x000169f2   0x00000002   PAD
    0x000169f4   0x000169f4   0x00000034   Code   RO         1453    i.drv_i2c_s_enable_intr  CVWL518.lib(drv_i2c_slave.o)
    0x00016a28   0x00016a28   0x0000001c   Code   RO         1454    i.drv_i2c_s_get_fifo_status  CVWL518.lib(drv_i2c_slave.o)
    0x00016a44   0x00016a44   0x0000000c   Code   RO         1457    i.drv_i2c_s_set_callback  CVWL518.lib(drv_i2c_slave.o)
    0x00016a50   0x00016a50   0x00000020   Code   RO         1460    i.drv_i2c_s_write_data  CVWL518.lib(drv_i2c_slave.o)
    0x00016a70   0x00016a70   0x00000050   Code   RO         1397    i.drv_i2c_set_dma_irq_callback  CVWL518.lib(drv_i2c_dma.o)
    0x00016ac0   0x00016ac0   0x00000044   Code   RO         1461    i.drv_i2c_slave_init  CVWL518.lib(drv_i2c_slave.o)
    0x00016b04   0x00016b04   0x00000024   Code   RO         1398    i.drv_i2c_slave_write_dma  CVWL518.lib(drv_i2c_dma.o)
    0x00016b28   0x00016b28   0x00000018   Code   RO         1926    i.drv_lcdc_config_420_to_444_mode  CVWL518.lib(drv_lcdc.o)
    0x00016b40   0x00016b40   0x00000018   Code   RO         1927    i.drv_lcdc_config_bypass  CVWL518.lib(drv_lcdc.o)
    0x00016b58   0x00016b58   0x00000018   Code   RO         1928    i.drv_lcdc_config_cbcr  CVWL518.lib(drv_lcdc.o)
    0x00016b70   0x00016b70   0x00000030   Code   RO         1929    i.drv_lcdc_config_ccm  CVWL518.lib(drv_lcdc.o)
    0x00016ba0   0x00016ba0   0x00000016   Code   RO         1930    i.drv_lcdc_config_disp_mode  CVWL518.lib(drv_lcdc.o)
    0x00016bb6   0x00016bb6   0x00000024   Code   RO         1931    i.drv_lcdc_config_dpi_polarity  CVWL518.lib(drv_lcdc.o)
    0x00016bda   0x00016bda   0x00000026   Code   RO         1932    i.drv_lcdc_config_dpi_timing  CVWL518.lib(drv_lcdc.o)
    0x00016c00   0x00016c00   0x00000016   Code   RO         1933    i.drv_lcdc_config_endianness  CVWL518.lib(drv_lcdc.o)
    0x00016c16   0x00016c16   0x00000020   Code   RO         1934    i.drv_lcdc_config_horiz_flip  CVWL518.lib(drv_lcdc.o)
    0x00016c36   0x00016c36   0x0000000c   Code   RO         1935    i.drv_lcdc_config_input_size  CVWL518.lib(drv_lcdc.o)
    0x00016c42   0x00016c42   0x0000001e   Code   RO         1936    i.drv_lcdc_config_int  CVWL518.lib(drv_lcdc.o)
    0x00016c60   0x00016c60   0x00000022   Code   RO         1937    i.drv_lcdc_config_int_single  CVWL518.lib(drv_lcdc.o)
    0x00016c82   0x00016c82   0x00000022   Code   RO         1938    i.drv_lcdc_config_overwrite  CVWL518.lib(drv_lcdc.o)
    0x00016ca4   0x00016ca4   0x0000000c   Code   RO         1939    i.drv_lcdc_config_overwrite_rgb  CVWL518.lib(drv_lcdc.o)
    0x00016cb0   0x00016cb0   0x0000001a   Code   RO         1940    i.drv_lcdc_config_partial_display_area  CVWL518.lib(drv_lcdc.o)
    0x00016cca   0x00016cca   0x00000022   Code   RO         1941    i.drv_lcdc_config_partial_display_enable  CVWL518.lib(drv_lcdc.o)
    0x00016cec   0x00016cec   0x00000072   Code   RO         1944    i.drv_lcdc_config_src_parameter  CVWL518.lib(drv_lcdc.o)
    0x00016d5e   0x00016d5e   0x00000008   Code   RO         1945    i.drv_lcdc_config_thresh  CVWL518.lib(drv_lcdc.o)
    0x00016d66   0x00016d66   0x00000060   Code   RO         1946    i.drv_lcdc_config_upscaler  CVWL518.lib(drv_lcdc.o)
    0x00016dc6   0x00016dc6   0x0000000a   Code   RO         1947    i.drv_lcdc_config_yuv420_threshold  CVWL518.lib(drv_lcdc.o)
    0x00016dd0   0x00016dd0   0x00000012   Code   RO         1948    i.drv_lcdc_ctrl_flow  CVWL518.lib(drv_lcdc.o)
    0x00016de2   0x00016de2   0x00000020   Code   RO         1950    i.drv_lcdc_enable_shadow_reg  CVWL518.lib(drv_lcdc.o)
    0x00016e02   0x00016e02   0x00000002   PAD
    0x00016e04   0x00016e04   0x00000034   Code   RO         1953    i.drv_lcdc_set_int  CVWL518.lib(drv_lcdc.o)
    0x00016e38   0x00016e38   0x00000020   Code   RO         1954    i.drv_lcdc_start    CVWL518.lib(drv_lcdc.o)
    0x00016e58   0x00016e58   0x0000000c   Code   RO         1955    i.drv_lcdc_update_shadow_reg  CVWL518.lib(drv_lcdc.o)
    0x00016e64   0x00016e64   0x00000010   Code   RO         1991    i.drv_memc_bypass_fifo_empty  CVWL518.lib(drv_memc.o)
    0x00016e74   0x00016e74   0x0000000c   Code   RO         1992    i.drv_memc_clear_status  CVWL518.lib(drv_memc.o)
    0x00016e80   0x00016e80   0x00000040   Code   RO         1993    i.drv_memc_enable_irq  CVWL518.lib(drv_memc.o)
    0x00016ec0   0x00016ec0   0x0000000c   Code   RO         1994    i.drv_memc_gen_a_tear_signal  CVWL518.lib(drv_memc.o)
    0x00016ecc   0x00016ecc   0x00000012   Code   RO         1995    i.drv_memc_get_status  CVWL518.lib(drv_memc.o)
    0x00016ede   0x00016ede   0x00000010   Code   RO         1996    i.drv_memc_rate_transfer_sel  CVWL518.lib(drv_memc.o)
    0x00016eee   0x00016eee   0x0000000e   Code   RO         1997    i.drv_memc_sel_vsync  CVWL518.lib(drv_memc.o)
    0x00016efc   0x00016efc   0x0000000c   Code   RO         1999    i.drv_memc_set_data_mode  CVWL518.lib(drv_memc.o)
    0x00016f08   0x00016f08   0x00000010   Code   RO         2002    i.drv_memc_set_tear_hwclr  CVWL518.lib(drv_memc.o)
    0x00016f18   0x00016f18   0x0000000e   Code   RO         2003    i.drv_memc_set_tear_mode  CVWL518.lib(drv_memc.o)
    0x00016f26   0x00016f26   0x00000002   PAD
    0x00016f28   0x00016f28   0x00000024   Code   RO         2004    i.drv_memc_set_tear_waveform  CVWL518.lib(drv_memc.o)
    0x00016f4c   0x00016f4c   0x00000010   Code   RO         2005    i.drv_memc_set_yuv420_cfg  CVWL518.lib(drv_memc.o)
    0x00016f5c   0x00016f5c   0x00000010   Code   RO         1482    i.drv_param_get_picture_quality_setting  CVWL518.lib(drv_param_init.o)
    0x00016f6c   0x00016f6c   0x00000008   Code   RO         1483    i.drv_param_init_get_ccm  CVWL518.lib(drv_param_init.o)
    0x00016f74   0x00016f74   0x00000014   Code   RO         1484    i.drv_param_init_get_scld_filter_h  CVWL518.lib(drv_param_init.o)
    0x00016f88   0x00016f88   0x00000014   Code   RO         1485    i.drv_param_init_get_scld_filter_v  CVWL518.lib(drv_param_init.o)
    0x00016f9c   0x00016f9c   0x00000008   Code   RO         1486    i.drv_param_init_get_sclu_filter_h  CVWL518.lib(drv_param_init.o)
    0x00016fa4   0x00016fa4   0x00000008   Code   RO         1487    i.drv_param_init_get_sclu_filter_v  CVWL518.lib(drv_param_init.o)
    0x00016fac   0x00016fac   0x00000014   Code   RO         1488    i.drv_param_init_set_ccm  CVWL518.lib(drv_param_init.o)
    0x00016fc0   0x00016fc0   0x0000003c   Code   RO         1491    i.drv_param_p2r_filter_init  CVWL518.lib(drv_param_init.o)
    0x00016ffc   0x00016ffc   0x00000034   Code   RO         1496    i.drv_param_yuv420_filter_init  CVWL518.lib(drv_param_init.o)
    0x00017030   0x00017030   0x00000060   Code   RO         2026    i.drv_phy_get_pll_para  CVWL518.lib(drv_phy_common.o)
    0x00017090   0x00017090   0x00000054   Code   RO         2027    i.drv_phy_get_rate_para  CVWL518.lib(drv_phy_common.o)
    0x000170e4   0x000170e4   0x00000010   Code   RO         2028    i.drv_phy_test_clear  CVWL518.lib(drv_phy_common.o)
    0x000170f4   0x000170f4   0x00000018   Code   RO         2029    i.drv_phy_test_lock  CVWL518.lib(drv_phy_common.o)
    0x0001710c   0x0001710c   0x00000020   Code   RO         2031    i.drv_phy_test_write_1_byte  CVWL518.lib(drv_phy_common.o)
    0x0001712c   0x0001712c   0x00000026   Code   RO         2032    i.drv_phy_test_write_2_byte  CVWL518.lib(drv_phy_common.o)
    0x00017152   0x00017152   0x0000001e   Code   RO         2033    i.drv_phy_test_write_code  CVWL518.lib(drv_phy_common.o)
    0x00017170   0x00017170   0x00000020   Code   RO         2034    i.drv_phy_test_write_data  CVWL518.lib(drv_phy_common.o)
    0x00017190   0x00017190   0x00000020   Code   RO         1529    i.drv_pwr_set_cp_mode  CVWL518.lib(drv_pwr.o)
    0x000171b0   0x000171b0   0x0000001c   Code   RO         1530    i.drv_pwr_set_pvd_mode  CVWL518.lib(drv_pwr.o)
    0x000171cc   0x000171cc   0x00000030   Code   RO         1531    i.drv_pwr_set_system_clk_src  CVWL518.lib(drv_pwr.o)
    0x000171fc   0x000171fc   0x0000000c   Code   RO         1780    i.drv_rx_phy_test_clear  CVWL518.lib(drv_dsi_rx.o)
    0x00017208   0x00017208   0x00000010   Code   RO         1781    i.drv_rx_phy_test_lock  CVWL518.lib(drv_dsi_rx.o)
    0x00017218   0x00017218   0x00000014   Code   RO         1783    i.drv_rx_phy_test_write_1_byte  CVWL518.lib(drv_dsi_rx.o)
    0x0001722c   0x0001722c   0x00000016   Code   RO         1784    i.drv_rx_phy_test_write_2_byte  CVWL518.lib(drv_dsi_rx.o)
    0x00017242   0x00017242   0x00000006   Code   RO         2049    i.drv_rxbr_clear_pkt_buffer  CVWL518.lib(drv_rxbr.o)
    0x00017248   0x00017248   0x00000004   Code   RO         2050    i.drv_rxbr_clear_status  CVWL518.lib(drv_rxbr.o)
    0x0001724c   0x0001724c   0x00000040   Code   RO         2052    i.drv_rxbr_enable_irq  CVWL518.lib(drv_rxbr.o)
    0x0001728c   0x0001728c   0x00000008   Code   RO         2054    i.drv_rxbr_frame_drop_cfg  CVWL518.lib(drv_rxbr.o)
    0x00017294   0x00017294   0x0000003c   Code   RO         2055    i.drv_rxbr_get_clk  CVWL518.lib(drv_rxbr.o)
    0x000172d0   0x000172d0   0x00000004   Code   RO         2056    i.drv_rxbr_get_col_addr  CVWL518.lib(drv_rxbr.o)
    0x000172d4   0x000172d4   0x00000008   Code   RO         2057    i.drv_rxbr_get_cur_hline_rcv_cnt  CVWL518.lib(drv_rxbr.o)
    0x000172dc   0x000172dc   0x00000010   Code   RO         2058    i.drv_rxbr_get_hline_rcv_cfg  CVWL518.lib(drv_rxbr.o)
    0x000172ec   0x000172ec   0x00000012   Code   RO         1694    i.drv_rxbr_get_int_source  CVWL518.lib(hal_internal_vsync.o)
    0x000172fe   0x000172fe   0x00000004   Code   RO         2060    i.drv_rxbr_get_page_addr  CVWL518.lib(drv_rxbr.o)
    0x00017302   0x00017302   0x00000012   Code   RO          594    i.drv_rxbr_get_status  CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x00017314   0x00017314   0x00000012   Code   RO         1695    i.drv_rxbr_get_status  CVWL518.lib(hal_internal_vsync.o)
    0x00017326   0x00017326   0x0000000c   Code   RO         2062    i.drv_rxbr_hline_rcv0_cfg  CVWL518.lib(drv_rxbr.o)
    0x00017332   0x00017332   0x00000008   Code   RO         2064    i.drv_rxbr_hline_rcv_cfg  CVWL518.lib(drv_rxbr.o)
    0x0001733a   0x0001733a   0x00000014   Code   RO         2066    i.drv_rxbr_set_ack_pkt_header  CVWL518.lib(drv_rxbr.o)
    0x0001734e   0x0001734e   0x000000cc   Code   RO         2067    i.drv_rxbr_set_cmd_filter  CVWL518.lib(drv_rxbr.o)
    0x0001741a   0x0001741a   0x00000014   Code   RO         2069    i.drv_rxbr_set_color_format  CVWL518.lib(drv_rxbr.o)
    0x0001742e   0x0001742e   0x00000014   Code   RO         2071    i.drv_rxbr_set_inten  CVWL518.lib(drv_rxbr.o)
    0x00017442   0x00017442   0x00000022   Code   RO         2073    i.drv_rxbr_set_usr_cfg  CVWL518.lib(drv_rxbr.o)
    0x00017464   0x00017464   0x00000008   Code   RO         2074    i.drv_rxbr_set_usr_col  CVWL518.lib(drv_rxbr.o)
    0x0001746c   0x0001746c   0x00000008   Code   RO         2075    i.drv_rxbr_set_usr_row  CVWL518.lib(drv_rxbr.o)
    0x00017474   0x00017474   0x00000020   Code   RO         1570    i.drv_spi_m_read_data  CVWL518.lib(drv_spi_master.o)
    0x00017494   0x00017494   0x00000048   Code   RO         1595    i.drv_swire_set_int  CVWL518.lib(drv_swire.o)
    0x000174dc   0x000174dc   0x0000001c   Code   RO         1596    i.drv_swire_set_power_down  CVWL518.lib(drv_swire.o)
    0x000174f8   0x000174f8   0x0000000c   Code   RO         1611    i.drv_sys_cfg_clear_all_int  CVWL518.lib(drv_sys_cfg.o)
    0x00017504   0x00017504   0x00000028   Code   RO         1612    i.drv_sys_cfg_clear_pending  CVWL518.lib(drv_sys_cfg.o)
    0x0001752c   0x0001752c   0x00000018   Code   RO         1615    i.drv_sys_cfg_sel_ap_rst_lvl_trig  CVWL518.lib(drv_sys_cfg.o)
    0x00017544   0x00017544   0x0000001c   Code   RO         1616    i.drv_sys_cfg_sel_ap_rst_trig  CVWL518.lib(drv_sys_cfg.o)
    0x00017560   0x00017560   0x00000024   Code   RO         1617    i.drv_sys_cfg_sel_gpio_group  CVWL518.lib(drv_sys_cfg.o)
    0x00017584   0x00017584   0x00000024   Code   RO         1618    i.drv_sys_cfg_sel_int_trig  CVWL518.lib(drv_sys_cfg.o)
    0x000175a8   0x000175a8   0x00000010   Code   RO         1620    i.drv_sys_cfg_set_dma_rx_req  CVWL518.lib(drv_sys_cfg.o)
    0x000175b8   0x000175b8   0x00000010   Code   RO         1621    i.drv_sys_cfg_set_dma_tx_req  CVWL518.lib(drv_sys_cfg.o)
    0x000175c8   0x000175c8   0x00000024   Code   RO         1622    i.drv_sys_cfg_set_int  CVWL518.lib(drv_sys_cfg.o)
    0x000175ec   0x000175ec   0x0000001a   Code   RO         1645    i.drv_timer_clear_status_flags  CVWL518.lib(drv_timer.o)
    0x00017606   0x00017606   0x00000020   Code   RO         1646    i.drv_timer_enable  CVWL518.lib(drv_timer.o)
    0x00017626   0x00017626   0x00000002   PAD
    0x00017628   0x00017628   0x00000010   Code   RO         1647    i.drv_timer_get_instance  CVWL518.lib(drv_timer.o)
    0x00017638   0x00017638   0x00000010   Code   RO         1648    i.drv_timer_get_prescaler  CVWL518.lib(drv_timer.o)
    0x00017648   0x00017648   0x0000003c   Code   RO         1650    i.drv_timer_handle_interrupt  CVWL518.lib(drv_timer.o)
    0x00017684   0x00017684   0x00000014   Code   RO         1651    i.drv_timer_register_callback  CVWL518.lib(drv_timer.o)
    0x00017698   0x00017698   0x00000010   Code   RO         1652    i.drv_timer_set_compare_val  CVWL518.lib(drv_timer.o)
    0x000176a8   0x000176a8   0x00000048   Code   RO         1653    i.drv_timer_set_int  CVWL518.lib(drv_timer.o)
    0x000176f0   0x000176f0   0x00000028   Code   RO         1654    i.drv_timer_set_prescaler  CVWL518.lib(drv_timer.o)
    0x00017718   0x00017718   0x0000000a   Code   RO         1861    i.drv_tx_phy_test_clear  CVWL518.lib(drv_dsi_tx.o)
    0x00017722   0x00017722   0x0000001c   Code   RO         1862    i.drv_tx_phy_test_enter  CVWL518.lib(drv_dsi_tx.o)
    0x0001773e   0x0001773e   0x0000001c   Code   RO         1863    i.drv_tx_phy_test_exit  CVWL518.lib(drv_dsi_tx.o)
    0x0001775a   0x0001775a   0x00000012   Code   RO         1865    i.drv_tx_phy_test_write_1_byte  CVWL518.lib(drv_dsi_tx.o)
    0x0001776c   0x0001776c   0x00000014   Code   RO         1866    i.drv_tx_phy_test_write_2_byte  CVWL518.lib(drv_dsi_tx.o)
    0x00017780   0x00017780   0x00000010   Code   RO         1867    i.drv_tx_phy_test_write_code  CVWL518.lib(drv_dsi_tx.o)
    0x00017790   0x00017790   0x00000008   Code   RO         2107    i.drv_vidc_clear_irq  CVWL518.lib(drv_vidc.o)
    0x00017798   0x00017798   0x00000018   Code   RO         2111    i.drv_vidc_enable   CVWL518.lib(drv_vidc.o)
    0x000177b0   0x000177b0   0x00000040   Code   RO         2112    i.drv_vidc_enable_irq  CVWL518.lib(drv_vidc.o)
    0x000177f0   0x000177f0   0x00000026   Code   RO         2113    i.drv_vidc_get_int_source  CVWL518.lib(drv_vidc.o)
    0x00017816   0x00017816   0x00000002   PAD
    0x00017818   0x00017818   0x00000044   Code   RO         2118    i.drv_vidc_module_enable  CVWL518.lib(drv_vidc.o)
    0x0001785c   0x0001785c   0x00000006   Code   RO         2119    i.drv_vidc_reset    CVWL518.lib(drv_vidc.o)
    0x00017862   0x00017862   0x0000005c   Code   RO         2121    i.drv_vidc_set_dst_parameter  CVWL518.lib(drv_vidc.o)
    0x000178be   0x000178be   0x0000000e   Code   RO         2122    i.drv_vidc_set_enh_chr  CVWL518.lib(drv_vidc.o)
    0x000178cc   0x000178cc   0x00000012   Code   RO         2123    i.drv_vidc_set_enh_chr2  CVWL518.lib(drv_vidc.o)
    0x000178de   0x000178de   0x0000000e   Code   RO         2124    i.drv_vidc_set_enh_lum  CVWL518.lib(drv_vidc.o)
    0x000178ec   0x000178ec   0x00000030   Code   RO         2126    i.drv_vidc_set_gain  CVWL518.lib(drv_vidc.o)
    0x0001791c   0x0001791c   0x00000014   Code   RO         2128    i.drv_vidc_set_irqen  CVWL518.lib(drv_vidc.o)
    0x00017930   0x00017930   0x00000008   Code   RO         2130    i.drv_vidc_set_p2r_hcoef0  CVWL518.lib(drv_vidc.o)
    0x00017938   0x00017938   0x00000008   Code   RO         2131    i.drv_vidc_set_p2r_hcoef1  CVWL518.lib(drv_vidc.o)
    0x00017940   0x00017940   0x00000028   Code   RO         2132    i.drv_vidc_set_p2r_hinitb  CVWL518.lib(drv_vidc.o)
    0x00017968   0x00017968   0x00000028   Code   RO         2133    i.drv_vidc_set_p2r_hinitr  CVWL518.lib(drv_vidc.o)
    0x00017990   0x00017990   0x00000008   Code   RO         2134    i.drv_vidc_set_p2r_step  CVWL518.lib(drv_vidc.o)
    0x00017998   0x00017998   0x00000020   Code   RO         2137    i.drv_vidc_set_pu_ctrl  CVWL518.lib(drv_vidc.o)
    0x000179b8   0x000179b8   0x0000000e   Code   RO         2138    i.drv_vidc_set_pu_scld  CVWL518.lib(drv_vidc.o)
    0x000179c6   0x000179c6   0x0000000a   Code   RO         2139    i.drv_vidc_set_scld_hcoef0  CVWL518.lib(drv_vidc.o)
    0x000179d0   0x000179d0   0x0000000a   Code   RO         2140    i.drv_vidc_set_scld_hcoef1  CVWL518.lib(drv_vidc.o)
    0x000179da   0x000179da   0x00000012   Code   RO         2141    i.drv_vidc_set_scld_step  CVWL518.lib(drv_vidc.o)
    0x000179ec   0x000179ec   0x0000000a   Code   RO         2142    i.drv_vidc_set_scld_vcoef0  CVWL518.lib(drv_vidc.o)
    0x000179f6   0x000179f6   0x0000000a   Code   RO         2143    i.drv_vidc_set_scld_vcoef1  CVWL518.lib(drv_vidc.o)
    0x00017a00   0x00017a00   0x0000000a   Code   RO         2144    i.drv_vidc_set_sclu_hcoef0c  CVWL518.lib(drv_vidc.o)
    0x00017a0a   0x00017a0a   0x0000000a   Code   RO         2145    i.drv_vidc_set_sclu_hcoef0y  CVWL518.lib(drv_vidc.o)
    0x00017a14   0x00017a14   0x0000000a   Code   RO         2146    i.drv_vidc_set_sclu_hcoef1c  CVWL518.lib(drv_vidc.o)
    0x00017a1e   0x00017a1e   0x0000000a   Code   RO         2147    i.drv_vidc_set_sclu_hcoef1y  CVWL518.lib(drv_vidc.o)
    0x00017a28   0x00017a28   0x0000000a   Code   RO         2148    i.drv_vidc_set_sclu_vcoef0c  CVWL518.lib(drv_vidc.o)
    0x00017a32   0x00017a32   0x0000000a   Code   RO         2149    i.drv_vidc_set_sclu_vcoef0y  CVWL518.lib(drv_vidc.o)
    0x00017a3c   0x00017a3c   0x0000000a   Code   RO         2150    i.drv_vidc_set_sclu_vcoef1c  CVWL518.lib(drv_vidc.o)
    0x00017a46   0x00017a46   0x0000000a   Code   RO         2151    i.drv_vidc_set_sclu_vcoef1y  CVWL518.lib(drv_vidc.o)
    0x00017a50   0x00017a50   0x00000024   Code   RO         2152    i.drv_vidc_set_src_parameter  CVWL518.lib(drv_vidc.o)
    0x00017a74   0x00017a74   0x0000000a   Code   RO         2153    i.drv_vidc_set_y4t2_hcoef0  CVWL518.lib(drv_vidc.o)
    0x00017a7e   0x00017a7e   0x0000000a   Code   RO         2154    i.drv_vidc_set_y4t2_hcoef1  CVWL518.lib(drv_vidc.o)
    0x00017a88   0x00017a88   0x0000000a   Code   RO         2156    i.drv_vidc_set_y4t2_vcoef0  CVWL518.lib(drv_vidc.o)
    0x00017a92   0x00017a92   0x0000000a   Code   RO         2157    i.drv_vidc_set_y4t2_vcoef1  CVWL518.lib(drv_vidc.o)
    0x00017a9c   0x00017a9c   0x00000010   Code   RO         2515    i.drv_wdg_clear_counter  CVWL518.lib(drv_wdg.o)
    0x00017aac   0x00017aac   0x00000010   Code   RO         2516    i.drv_wdg_clear_edge_flag  CVWL518.lib(drv_wdg.o)
    0x00017abc   0x00017abc   0x00000010   Code   RO         2519    i.drv_wdg_read_edge_flag  CVWL518.lib(drv_wdg.o)
    0x00017acc   0x00017acc   0x00000034   Code   RO         2522    i.drv_wdg_set_int   CVWL518.lib(drv_wdg.o)
    0x00017b00   0x00017b00   0x00000006   Code   RO         1260    i.fls_clear_irq_status  CVWL518.lib(drv_fls.o)
    0x00017b06   0x00017b06   0x00000014   Code   RO          980    i.fputc             CVWL518.lib(tau_log.o)
    0x00017b1a   0x00017b1a   0x00000002   PAD
    0x00017b1c   0x00017b1c   0x00000030   Code   RO          597    i.hal_dsi_rx_ctrl_create_handle  CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x00017b4c   0x00017b4c   0x0000009c   Code   RO          598    i.hal_dsi_rx_ctrl_deinit  CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x00017be8   0x00017be8   0x00000084   Code   RO          599    i.hal_dsi_rx_ctrl_dsc_async_handler  CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x00017c6c   0x00017c6c   0x00000028   Code   RO          601    i.hal_dsi_rx_ctrl_gen_a_tear_signal  CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x00017c94   0x00017c94   0x00000028   Code   RO          603    i.hal_dsi_rx_ctrl_get_max_ret_size  CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x00017cbc   0x00017cbc   0x00000064   Code   RO          605    i.hal_dsi_rx_ctrl_init  CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x00017d20   0x00017d20   0x00000124   Code   RO          606    i.hal_dsi_rx_ctrl_init_clk  CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x00017e44   0x00017e44   0x00000048   Code   RO          607    i.hal_dsi_rx_ctrl_init_dsc_dec  CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x00017e8c   0x00017e8c   0x000000cc   Code   RO          608    i.hal_dsi_rx_ctrl_init_dsi_rx  CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x00017f58   0x00017f58   0x000000c4   Code   RO          609    i.hal_dsi_rx_ctrl_init_memc  CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x0001801c   0x0001801c   0x0000014c   Code   RO          610    i.hal_dsi_rx_ctrl_init_rxbr  CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x00018168   0x00018168   0x00000388   Code   RO          611    i.hal_dsi_rx_ctrl_init_vidc  CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x000184f0   0x000184f0   0x0000003c   Code   RO          612    i.hal_dsi_rx_ctrl_pre_init_pps  CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x0001852c   0x0001852c   0x000000f0   Code   RO          615    i.hal_dsi_rx_ctrl_send_ack_cmd  CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x0001861c   0x0001861c   0x00000034   Code   RO          623    i.hal_dsi_rx_ctrl_set_cus_sync_line  CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x00018650   0x00018650   0x00000034   Code   RO          626    i.hal_dsi_rx_ctrl_set_hw_tear_mode  CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x00018684   0x00018684   0x00000034   Code   RO          627    i.hal_dsi_rx_ctrl_set_ipi_cfg  CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x000186b8   0x000186b8   0x00000072   Code   RO          630    i.hal_dsi_rx_ctrl_set_rxbr_clk  CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x0001872a   0x0001872a   0x00000002   PAD
    0x0001872c   0x0001872c   0x00000034   Code   RO          631    i.hal_dsi_rx_ctrl_set_sw_tear_mode  CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x00018760   0x00018760   0x0000003c   Code   RO          634    i.hal_dsi_rx_ctrl_start  CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x0001879c   0x0001879c   0x00000048   Code   RO          635    i.hal_dsi_rx_ctrl_stop  CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x000187e4   0x000187e4   0x00000020   Code   RO          637    i.hal_dsi_rx_ctrl_toggle_resolution  CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x00018804   0x00018804   0x00000190   Code   RO          689    i.hal_dsi_tx_calc_video_chunks  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x00018994   0x00018994   0x00000034   Code   RO          690    i.hal_dsi_tx_config_params_for_lane_rate  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x000189c8   0x000189c8   0x000003c0   Code   RO          691    i.hal_dsi_tx_count_lane_rate  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x00018d88   0x00018d88   0x0000002c   Code   RO          693    i.hal_dsi_tx_ctrl_create_handle  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x00018db4   0x00018db4   0x00000048   Code   RO          694    i.hal_dsi_tx_ctrl_deinit  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x00018dfc   0x00018dfc   0x0000004c   Code   RO          695    i.hal_dsi_tx_ctrl_enter_init_panel_mode  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x00018e48   0x00018e48   0x00000024   Code   RO          697    i.hal_dsi_tx_ctrl_exit_init_panel_mode  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x00018e6c   0x00018e6c   0x000000c4   Code   RO          699    i.hal_dsi_tx_ctrl_init  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x00018f30   0x00018f30   0x00000024   Code   RO          700    i.hal_dsi_tx_ctrl_init_clk  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x00018f54   0x00018f54   0x0000000c   Code   RO          701    i.hal_dsi_tx_ctrl_panel_reset_pin  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x00018f60   0x00018f60   0x00000020   Code   RO          704    i.hal_dsi_tx_ctrl_set_ccm  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x00018f80   0x00018f80   0x00000014   Code   RO          712    i.hal_dsi_tx_ctrl_set_overwrite_rgb  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x00018f94   0x00018f94   0x00000010   Code   RO          713    i.hal_dsi_tx_ctrl_set_partial_disp  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x00018fa4   0x00018fa4   0x00000024   Code   RO          714    i.hal_dsi_tx_ctrl_set_partial_disp_area  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x00018fc8   0x00018fc8   0x00000060   Code   RO          716    i.hal_dsi_tx_ctrl_start  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x00019028   0x00019028   0x00000044   Code   RO          717    i.hal_dsi_tx_ctrl_stop  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x0001906c   0x0001906c   0x0000019c   Code   RO          718    i.hal_dsi_tx_ctrl_write_array_cmd  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x00019208   0x00019208   0x00000150   Code   RO          719    i.hal_dsi_tx_ctrl_write_cmd  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x00019358   0x00019358   0x00000028   Code   RO          720    i.hal_dsi_tx_init_data_mode  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x00019380   0x00019380   0x00000030   Code   RO          721    i.hal_dsi_tx_init_dpi_cfg  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x000193b0   0x000193b0   0x00000020   Code   RO          722    i.hal_dsi_tx_init_interrupt  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x000193d0   0x000193d0   0x00000020   Code   RO          723    i.hal_dsi_tx_init_phy_cfg  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x000193f0   0x000193f0   0x00000094   Code   RO          724    i.hal_dsi_tx_init_remains  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x00019484   0x00019484   0x00000058   Code   RO          725    i.hal_dsi_tx_init_video_mode  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x000194dc   0x000194dc   0x00000044   Code   RO          726    i.hal_dsi_tx_send_cmd  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x00019520   0x00019520   0x00000018   Code   RO          787    i.hal_gpio_ctrl_eint  CVWL518.lib(hal_gpio.o)
    0x00019538   0x00019538   0x00000012   Code   RO          788    i.hal_gpio_get_input_data  CVWL518.lib(hal_gpio.o)
    0x0001954a   0x0001954a   0x00000002   PAD
    0x0001954c   0x0001954c   0x00000040   Code   RO          791    i.hal_gpio_init_eint  CVWL518.lib(hal_gpio.o)
    0x0001958c   0x0001958c   0x00000020   Code   RO          792    i.hal_gpio_init_input  CVWL518.lib(hal_gpio.o)
    0x000195ac   0x000195ac   0x00000028   Code   RO          793    i.hal_gpio_init_output  CVWL518.lib(hal_gpio.o)
    0x000195d4   0x000195d4   0x00000018   Code   RO          794    i.hal_gpio_reg_eint_cb  CVWL518.lib(hal_gpio.o)
    0x000195ec   0x000195ec   0x00000050   Code   RO          795    i.hal_gpio_set_ap_reset_int  CVWL518.lib(hal_gpio.o)
    0x0001963c   0x0001963c   0x00000060   Code   RO          797    i.hal_gpio_set_mode  CVWL518.lib(hal_gpio.o)
    0x0001969c   0x0001969c   0x00000008   Code   RO          798    i.hal_gpio_set_output_data  CVWL518.lib(hal_gpio.o)
    0x000196a4   0x000196a4   0x00000020   Code   RO          800    i.hal_gpio_set_pull_state  CVWL518.lib(hal_gpio.o)
    0x000196c4   0x000196c4   0x0000006c   Code   RO          826    i.hal_i2c_m_dma_init  CVWL518.lib(hal_i2c_master.o)
    0x00019730   0x00019730   0x0000002c   Code   RO          827    i.hal_i2c_m_dma_read  CVWL518.lib(hal_i2c_master.o)
    0x0001975c   0x0001975c   0x00000028   Code   RO          828    i.hal_i2c_m_dma_write  CVWL518.lib(hal_i2c_master.o)
    0x00019784   0x00019784   0x00000020   Code   RO          830    i.hal_i2c_m_transfer_complate  CVWL518.lib(hal_i2c_master.o)
    0x000197a4   0x000197a4   0x00000020   Code   RO          831    i.hal_i2c_master_irq_callback  CVWL518.lib(hal_i2c_master.o)
    0x000197c4   0x000197c4   0x00000010   Code   RO          845    i.hal_i2c_s_dma_user_callback  CVWL518.lib(hal_i2c_slave.o)
    0x000197d4   0x000197d4   0x0000003c   Code   RO          846    i.hal_i2c_s_dma_write  CVWL518.lib(hal_i2c_slave.o)
    0x00019810   0x00019810   0x0000006c   Code   RO          848    i.hal_i2c_s_init    CVWL518.lib(hal_i2c_slave.o)
    0x0001987c   0x0001987c   0x00000014   Code   RO          849    i.hal_i2c_s_nonblocking_read  CVWL518.lib(hal_i2c_slave.o)
    0x00019890   0x00019890   0x0000000c   Code   RO          856    i.hal_i2c_s_set_transfer  CVWL518.lib(hal_i2c_slave.o)
    0x0001989c   0x0001989c   0x00000150   Code   RO          859    i.hal_i2c_slave_irq_callback  CVWL518.lib(hal_i2c_slave.o)
    0x000199ec   0x000199ec   0x000000b0   Code   RO         1696    i.hal_internal_init_memc  CVWL518.lib(hal_internal_vsync.o)
    0x00019a9c   0x00019a9c   0x00000010   Code   RO         1697    i.hal_internal_sync_get_fb_setting  CVWL518.lib(hal_internal_vsync.o)
    0x00019aac   0x00019aac   0x0000024c   Code   RO         1698    i.hal_internal_sync_input_resolution_change  CVWL518.lib(hal_internal_vsync.o)
    0x00019cf8   0x00019cf8   0x00000188   Code   RO         1699    i.hal_internal_sync_set_fb_setting_manual  CVWL518.lib(hal_internal_vsync.o)
    0x00019e80   0x00019e80   0x0000001c   Code   RO         1700    i.hal_internal_vsync_deinit  CVWL518.lib(hal_internal_vsync.o)
    0x00019e9c   0x00019e9c   0x0000000c   Code   RO         1701    i.hal_internal_vsync_get_rx_state  CVWL518.lib(hal_internal_vsync.o)
    0x00019ea8   0x00019ea8   0x0000001c   Code   RO         1702    i.hal_internal_vsync_get_sync_line  CVWL518.lib(hal_internal_vsync.o)
    0x00019ec4   0x00019ec4   0x0000000c   Code   RO         1703    i.hal_internal_vsync_get_tx_state  CVWL518.lib(hal_internal_vsync.o)
    0x00019ed0   0x00019ed0   0x00000020   Code   RO         1704    i.hal_internal_vsync_get_y2t4_use_sclu  CVWL518.lib(hal_internal_vsync.o)
    0x00019ef0   0x00019ef0   0x000000bc   Code   RO         1705    i.hal_internal_vsync_init_rx  CVWL518.lib(hal_internal_vsync.o)
    0x00019fac   0x00019fac   0x000000a4   Code   RO         1706    i.hal_internal_vsync_init_tx  CVWL518.lib(hal_internal_vsync.o)
    0x0001a050   0x0001a050   0x0000011c   Code   RO         1707    i.hal_internal_vsync_set_auto_hw_filter  CVWL518.lib(hal_internal_vsync.o)
    0x0001a16c   0x0001a16c   0x00000018   Code   RO         1709    i.hal_internal_vsync_set_rx_state  CVWL518.lib(hal_internal_vsync.o)
    0x0001a184   0x0001a184   0x00000020   Code   RO         1710    i.hal_internal_vsync_set_sync_line  CVWL518.lib(hal_internal_vsync.o)
    0x0001a1a4   0x0001a1a4   0x00000048   Code   RO         1711    i.hal_internal_vsync_set_tear_mode  CVWL518.lib(hal_internal_vsync.o)
    0x0001a1ec   0x0001a1ec   0x00000044   Code   RO         1712    i.hal_internal_vsync_set_tx_state  CVWL518.lib(hal_internal_vsync.o)
    0x0001a230   0x0001a230   0x00000024   Code   RO          727    i.hal_lcdc_config_ccm  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x0001a254   0x0001a254   0x00000054   Code   RO          728    i.hal_lcdc_config_remains  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x0001a2a8   0x0001a2a8   0x00000014   Code   RO          729    i.hal_lcdc_config_rgb_to_pentile  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x0001a2bc   0x0001a2bc   0x000001c8   Code   RO          730    i.hal_lcdc_config_upscaler  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x0001a484   0x0001a484   0x00000020   Code   RO          731    i.hal_lcdc_config_yuv_to_rgb  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x0001a4a4   0x0001a4a4   0x0000003a   Code   RO          732    i.hal_lcdc_init_cfg  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x0001a4de   0x0001a4de   0x00000002   PAD
    0x0001a4e0   0x0001a4e0   0x00000180   Code   RO          733    i.hal_lcdc_init_clk  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x0001a660   0x0001a660   0x00000040   Code   RO          734    i.hal_lcdc_init_interrupt  CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x0001a6a0   0x0001a6a0   0x0000000e   Code   RO          882    i.hal_spi_m_clear_rxfifo  CVWL518.lib(hal_spi_master.o)
    0x0001a6ae   0x0001a6ae   0x00000016   Code   RO          906    i.hal_swire_open    CVWL518.lib(hal_swire.o)
    0x0001a6c4   0x0001a6c4   0x00000008   Code   RO          920    i.hal_system_enable_systick  CVWL518.lib(hal_system.o)
    0x0001a6cc   0x0001a6cc   0x00000088   Code   RO          925    i.hal_system_init   CVWL518.lib(hal_system.o)
    0x0001a754   0x0001a754   0x0000001c   Code   RO          926    i.hal_system_init_console  CVWL518.lib(hal_system.o)
    0x0001a770   0x0001a770   0x00000008   Code   RO          929    i.hal_system_set_pvd  CVWL518.lib(hal_system.o)
    0x0001a778   0x0001a778   0x00000008   Code   RO          930    i.hal_system_set_vcc  CVWL518.lib(hal_system.o)
    0x0001a780   0x0001a780   0x0000001a   Code   RO          954    i.hal_timer_init    CVWL518.lib(hal_timer.o)
    0x0001a79a   0x0001a79a   0x00000002   PAD
    0x0001a79c   0x0001a79c   0x00000048   Code   RO          956    i.hal_timer_start   CVWL518.lib(hal_timer.o)
    0x0001a7e4   0x0001a7e4   0x00000028   Code   RO          958    i.hal_timer_stop    CVWL518.lib(hal_timer.o)
    0x0001a80c   0x0001a80c   0x0000008c   Code   RO         1075    i.hal_uart_init     CVWL518.lib(hal_uart.o)
    0x0001a898   0x0001a898   0x00000010   Code   RO         1078    i.hal_uart_transmit_blocking  CVWL518.lib(hal_uart.o)
    0x0001a8a8   0x0001a8a8   0x00000108   Code   RO         2250    i.handle_init       CVWL518.lib(irq_redirect .o)
    0x0001a9b0   0x0001a9b0   0x00000068   Code   RO          114    i.init_mipi_tx      ap_demo.o
    0x0001aa18   0x0001aa18   0x000000b8   Code   RO          115    i.init_panel        ap_demo.o
    0x0001aad0   0x0001aad0   0x0000000a   Code   RO            3    i.main              main.o
    0x0001aada   0x0001aada   0x00000002   PAD
    0x0001aadc   0x0001aadc   0x000000a4   Code   RO          116    i.open_mipi_rx      ap_demo.o
    0x0001ab80   0x0001ab80   0x00000054   Code   RO          117    i.pps_update_handle  ap_demo.o
    0x0001abd4   0x0001abd4   0x00000410   Code   RO         1713    i.rx_get_dcs_packet_data  CVWL518.lib(hal_internal_vsync.o)
    0x0001afe4   0x0001afe4   0x0000013c   Code   RO         1714    i.rx_partial_update  CVWL518.lib(hal_internal_vsync.o)
    0x0001b120   0x0001b120   0x00000064   Code   RO         1715    i.rx_receive_packet  CVWL518.lib(hal_internal_vsync.o)
    0x0001b184   0x0001b184   0x00000180   Code   RO         1716    i.rx_receive_pps    CVWL518.lib(hal_internal_vsync.o)
    0x0001b304   0x0001b304   0x0000002a   Code   RO          118    i.send_panel_init_code  ap_demo.o
    0x0001b32e   0x0001b32e   0x00000002   PAD
    0x0001b330   0x0001b330   0x00000060   Code   RO          119    i.soft_disable_mipi_timer_init  ap_demo.o
    0x0001b390   0x0001b390   0x0000008c   Code   RO         1717    i.soft_gen_te       CVWL518.lib(hal_internal_vsync.o)
    0x0001b41c   0x0001b41c   0x00000030   Code   RO          120    i.soft_timer3_cb    ap_demo.o
    0x0001b44c   0x0001b44c   0x00000048   Code   RO          121    i.tp_heartbeat_exec  ap_demo.o
    0x0001b494   0x0001b494   0x00000014   Code   RO          122    i.tx_display_on     ap_demo.o
    0x0001b4a8   0x0001b4a8   0x00000028   Code   RO          123    i.tx_panel_reset    ap_demo.o
    0x0001b4d0   0x0001b4d0   0x000000d0   Code   RO         1718    i.vpre_err_reset    CVWL518.lib(hal_internal_vsync.o)
    0x0001b5a0   0x0001b5a0   0x0000019c   Code   RO         1719    i.vsync_set_te_mode  CVWL518.lib(hal_internal_vsync.o)
    0x0001b73c   0x0001b73c   0x000000ec   Data   RO          124    .constdata          ap_demo.o
    0x0001b828   0x0001b828   0x00002150   Data   RO          292    .constdata          app_tp_for_custom_s8.o
    0x0001d978   0x0001d978   0x000000d2   Data   RO          803    .constdata          CVWL518.lib(hal_gpio.o)
    0x0001da4a   0x0001da4a   0x00000002   PAD
    0x0001da4c   0x0001da4c   0x00000110   Data   RO         1497    .constdata          CVWL518.lib(drv_param_init.o)
    0x0001db5c   0x0001db5c   0x00000186   Data   RO         2035    .constdata          CVWL518.lib(drv_phy_common.o)
    0x0001dce2   0x0001dce2   0x00000002   PAD
    0x0001dce4   0x0001dce4   0x00000048   Data   RO          639    .conststring        CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x0001dd2c   0x0001dd2c   0x00000128   Data   RO         1721    .conststring        CVWL518.lib(hal_internal_vsync.o)
    0x0001de54   0x0001de54   0x00000030   Data   RO         2910    Region$$Table       anon$$obj.o


    Execution Region RW_RAM1 (Exec base: 0x00070000, Load base: 0x0001de84, Size: 0x00000000, Max: 0x000000f0, ABSOLUTE)

    **** No section assigned to this execution region ****


    Execution Region RW_RAM2 (Exec base: 0x00070100, Load base: 0x0001de84, Size: 0x000000c0, Max: 0x000000d0, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00070100        -       0x000000c0   Zero   RW         2251    .ARM.__AT_0x00070100  CVWL518.lib(irq_redirect .o)


    Execution Region RW_RAM3 (Exec base: 0x000701d0, Load base: 0x0001de84, Size: 0x00005840, Max: 0x00007e30, ABSOLUTE, COMPRESSED[0x00001f28])

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x000701d0   COMPRESSED   0x00002719   Data   RW          125    .data               ap_demo.o
    0x000728e9   COMPRESSED   0x00000001   PAD
    0x000728ea   COMPRESSED   0x000000e4   Data   RW          306    .data               app_tp_for_custom_s8.o
    0x000729ce   COMPRESSED   0x00000001   Data   RW          309    .data               app_tp_for_custom_s8.o
    0x000729cf   COMPRESSED   0x00000001   Data   RW          310    .data               app_tp_for_custom_s8.o
    0x000729d0   COMPRESSED   0x00000001   Data   RW          315    .data               app_tp_for_custom_s8.o
    0x000729d1   COMPRESSED   0x00000003   Data   RW          316    .data               app_tp_for_custom_s8.o
    0x000729d4   COMPRESSED   0x00000005   Data   RW          317    .data               app_tp_for_custom_s8.o
    0x000729d9   COMPRESSED   0x00000003   PAD
    0x000729dc   COMPRESSED   0x00000030   Data   RW          327    .data               app_tp_for_custom_s8.o
    0x00072a0c   COMPRESSED   0x00000031   Data   RW          403    .data               app_tp_transfer.o
    0x00072a3d   COMPRESSED   0x00000003   PAD
    0x00072a40   COMPRESSED   0x00000008   Data   RW          640    .data               CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x00072a48   COMPRESSED   0x00000001   Data   RW          832    .data               CVWL518.lib(hal_i2c_master.o)
    0x00072a49   COMPRESSED   0x00000003   PAD
    0x00072a4c   COMPRESSED   0x0000001c   Data   RW          860    .data               CVWL518.lib(hal_i2c_slave.o)
    0x00072a68   COMPRESSED   0x00000012   Data   RW         1029    .data               CVWL518.lib(norflash.o)
    0x00072a7a   COMPRESSED   0x00000002   PAD
    0x00072a7c   COMPRESSED   0x0000000c   Data   RW         1102    .data               CVWL518.lib(drv_common.o)
    0x00072a88   COMPRESSED   0x00000004   Data   RW         1362    .data               CVWL518.lib(drv_gpio.o)
    0x00072a8c   COMPRESSED   0x00000008   Data   RW         1400    .data               CVWL518.lib(drv_i2c_dma.o)
    0x00072a94   COMPRESSED   0x00000004   Data   RW         1428    .data               CVWL518.lib(drv_i2c_master.o)
    0x00072a98   COMPRESSED   0x00000008   Data   RW         1462    .data               CVWL518.lib(drv_i2c_slave.o)
    0x00072aa0   COMPRESSED   0x0000064c   Data   RW         1498    .data               CVWL518.lib(drv_param_init.o)
    0x000730ec   COMPRESSED   0x00000004   Data   RW         1574    .data               CVWL518.lib(drv_spi_master.o)
    0x000730f0   COMPRESSED   0x00000008   Data   RW         1598    .data               CVWL518.lib(drv_swire.o)
    0x000730f8   COMPRESSED   0x00000001   Data   RW         1623    .data               CVWL518.lib(drv_sys_cfg.o)
    0x000730f9   COMPRESSED   0x00000003   PAD
    0x000730fc   COMPRESSED   0x00000050   Data   RW         1656    .data               CVWL518.lib(drv_timer.o)
    0x0007314c   COMPRESSED   0x00000004   Data   RW         1722    .data               CVWL518.lib(hal_internal_vsync.o)
    0x00073150   COMPRESSED   0x00000008   Data   RW         2293    .data               CVWL518.lib(drv_chip_info.o)
    0x00073158   COMPRESSED   0x0000000c   Data   RW         2405    .data               CVWL518.lib(drv_pwm.o)
    0x00073164   COMPRESSED   0x00000008   Data   RW         2457    .data               CVWL518.lib(drv_uart.o)
    0x0007316c   COMPRESSED   0x0000000c   Data   RW         2524    .data               CVWL518.lib(drv_wdg.o)
    0x00073178   COMPRESSED   0x00000004   Data   RW         2884    .data               mc_p.l(stdout.o)
    0x0007317c        -       0x0000019c   Zero   RW          402    .bss                app_tp_transfer.o
    0x00073318        -       0x000000b8   Zero   RW          638    .bss                CVWL518.lib(hal_dsi_rx_ctrl.o)
    0x000733d0        -       0x00000040   Zero   RW          735    .bss                CVWL518.lib(hal_dsi_tx_ctrl.o)
    0x00073410        -       0x00000100   Zero   RW          981    .bss                CVWL518.lib(tau_log.o)
    0x00073510        -       0x0000003c   Zero   RW         1080    .bss                CVWL518.lib(hal_uart.o)
    0x0007354c        -       0x00000018   Zero   RW         1226    .bss                CVWL518.lib(drv_dma.o)
    0x00073564        -       0x00000040   Zero   RW         1361    .bss                CVWL518.lib(drv_gpio.o)
    0x000735a4        -       0x00000018   Zero   RW         1399    .bss                CVWL518.lib(drv_i2c_dma.o)
    0x000735bc        -       0x00000acc   Zero   RW         1679    .bss                CVWL518.lib(dcs_packet_fifo.o)
    0x00074088        -       0x00000968   Zero   RW         1720    .bss                CVWL518.lib(hal_internal_vsync.o)
    0x000749f0        -       0x00000020   Zero   RW         2337    .bss                CVWL518.lib(hal_spi_slave.o)
    0x00074a10        -       0x00001000   Zero   RW          585    STACK               startup_armcm0.o


==============================================================================

Image component sizes


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Object Name

      8202        846        236      10009          0      38740   ap_demo.o
      1756         72       8529        287          0      13583   app_tp_for_custom_s8.o
      1778        210          0         49        412      17388   app_tp_transfer.o
        28          4          0          0          0        445   board.o
        10          0          0          0          0      10151   main.o
       120         18        192          0       4096       2028   startup_armcm0.o

    ----------------------------------------------------------------------
     11902       1150       9006      10352       4508      82335   Object Totals
         0          0         48          0          0          0   (incl. Generated)
         8          0          1          7          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Member Name

       216         32          0          0       2764        252   dcs_packet_fifo.o
       300         66          0          8          0        264   drv_chip_info.o
       232         96         20         12          0        264   drv_common.o
       420         90          0          0          0       1200   drv_crgu.o
       478         68          0          0         24        856   drv_dma.o
       296         34          0          0          0        344   drv_dsc_dec.o
      1454        496          0          0          0       1260   drv_dsi_rx.o
      1432        118          0          0          0       2364   drv_dsi_tx.o
         6          0          0          0          0         60   drv_fls.o
       784        112          0          4         64       1236   drv_gpio.o
       624         78          0          8         24        624   drv_i2c_dma.o
       344         80          0          4          0        396   drv_i2c_master.o
       324         74          0          8          0        516   drv_i2c_slave.o
       826          6          0          0          0       1588   drv_lcdc.o
       342         18          0          0          0        804   drv_memc.o
       212         48        272       1612          0        592   drv_param_init.o
       352         16        390          0          0        532   drv_phy_common.o
        72         10          0         12          0         76   drv_pwm.o
       108         22          0          0          0        180   drv_pwr.o
       508         38          0          0          0       1136   drv_rxbr.o
        64         14          0          4          0        128   drv_spi_master.o
       132         16          0          8          0        200   drv_swire.o
       300         64          0          1          0        628   drv_sys_cfg.o
       338         30          0         80          0        872   drv_timer.o
       698         18          0          8          0        680   drv_uart.o
       778         16          0          0          0       2312   drv_vidc.o
       156         22          0         12          0        316   drv_wdg.o
      3320        306         72          8        184       1660   hal_dsi_rx_ctrl.o
      4490        212          0          0         64       2444   hal_dsi_tx_ctrl.o
       450         48        210          0          0        752   hal_gpio.o
       256         48          0          1          0        340   hal_i2c_master.o
       552         70          0         28          0        400   hal_i2c_slave.o
      6456       1370        296          4       2408       2324   hal_internal_vsync.o
        14          0          0          0          0         68   hal_spi_master.o
       580         32          0          0         32        136   hal_spi_slave.o
        22          0          0          0          0         68   hal_swire.o
       188         32          0          0          0        340   hal_system.o
       138          6          0          0          0        208   hal_timer.o
       156         18          0          0         60        144   hal_uart.o
      1072        320          0          0        192       1980   irq_redirect .o
        48         10          0         18          0         68   norflash.o
        58          0          0          0          0        128   tau_delay.o
        60         10          0          0        256        156   tau_log.o
       200         20          0          0          0         76   ceil.o
        86          0          0          0          0          0   __dczerorl2.o
         0          0          0          0          0          0   entry.o
         0          0          0          0          0          0   entry10a.o
         0          0          0          0          0          0   entry11a.o
         8          4          0          0          0          0   entry2.o
         4          0          0          0          0          0   entry5.o
         0          0          0          0          0          0   entry7b.o
         0          0          0          0          0          0   entry8b.o
         8          4          0          0          0          0   entry9a.o
        30          0          0          0          0          0   handlers.o
        40          0          0          0          0         72   idiv.o
        36          8          0          0          0         68   init.o
         0          0          0          0          0          0   iusefp.o
        32          0          0          0          0         68   llshl.o
        38          0          0          0          0         68   llsshr.o
        34          0          0          0          0         68   llushr.o
        36          0          0          0          0         60   memcpya.o
        36          0          0          0          0        100   memseta.o
      2298        104          0          0          0        544   printfa.o
         0          0          0          4          0          0   stdout.o
        44          0          0          0          0         72   uidiv.o
        96          0          0          0          0         84   uldiv.o
        40          2          0          0          0         68   cdrcmple.o
        20          0          0          0          0         68   cfrcmple.o
       356          4          0          0          0        140   dadd.o
       240          6          0          0          0         84   ddiv.o
       236          0          0          0          0        216   depilogue.o
        72         10          0          0          0         72   dfixi.o
        60         10          0          0          0         68   dfixui.o
        64         10          0          0          0         68   dfixul.o
        28          4          0          0          0         68   dfltui.o
       208          6          0          0          0         88   dmul.o
        40          0          0          0          0         60   f2d.o
       178          0          0          0          0        108   fadd.o
       124          0          0          0          0         72   fdiv.o
       130          0          0          0          0        144   fepilogue.o
        50          0          0          0          0         60   ffixi.o
        40          0          0          0          0         60   ffixui.o
        22          0          0          0          0         68   fflti.o
        14          0          0          0          0         68   ffltui.o
       122          0          0          0          0         72   fmul.o
        24          0          0          0          0         60   fscalb.o

    ----------------------------------------------------------------------
     34792       4356       1264       1852       6072      33888   Library Totals
        42          0          4          8          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Name

     29656       4164       1260       1840       6072      30896   CVWL518.lib
       200         20          0          0          0         76   m_ps.l
      2826        120          0          4          0       1204   mc_p.l
      2068         52          0          0          0       1712   mf_p.l

    ----------------------------------------------------------------------
     34792       4356       1264       1852       6072      33888   Library Totals

    ----------------------------------------------------------------------

==============================================================================


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   

     46694       5506      10270      12204      10580      92099   Grand Totals
     46694       5506      10270       7976      10580      92099   ELF Image Totals (compressed)
     46694       5506      10270       7976          0          0   ROM Totals

==============================================================================

    Total RO  Size (Code + RO Data)                56964 (  55.63kB)
    Total RW  Size (RW Data + ZI Data)             22784 (  22.25kB)
    Total ROM Size (Code + RO Data + RW Data)      64940 (  63.42kB)

==============================================================================

