Component: ARM Compiler 5.06 update 6 (build 750) Tool: armlink [4d35ed]

==============================================================================

Section Cross References

    main.o(i.main) refers to board.o(i.board_Init) for board_Init
    main.o(i.main) refers to ap_demo.o(i.ap_demo) for ap_demo
    ap_demo.o(i.Gpio_swire_output) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    ap_demo.o(i.Gpio_swire_output) refers to tau_delay.o(i.delayUs) for delayUs
    ap_demo.o(i.Gpio_swire_output) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    ap_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) for hal_dsi_rx_ctrl_get_max_ret_size
    ap_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) for hal_dsi_rx_ctrl_send_ack_cmd
    ap_demo.o(i.ap_dcs_read) refers to app_tp_st_touch.o(i.ap_get_tp_calibration_status_01) for ap_get_tp_calibration_status_01
    ap_demo.o(i.ap_dcs_read) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_demo) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_I2C_init) for app_tp_I2C_init
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.open_mipi_rx) for open_mipi_rx
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.init_mipi_tx) for init_mipi_tx
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_init) for app_tp_init
    ap_demo.o(i.ap_demo) refers to hal_timer.o(i.hal_timer_init) for hal_timer_init
    ap_demo.o(i.ap_demo) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.init_panel) for init_panel
    ap_demo.o(i.ap_demo) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    ap_demo.o(i.ap_demo) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.ap_demo) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.Gpio_swire_output) for Gpio_swire_output
    ap_demo.o(i.ap_demo) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_phone_clear_reset_on) for app_tp_phone_clear_reset_on
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_transfer_screen_start) for app_tp_transfer_screen_start
    ap_demo.o(i.ap_demo) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) for hal_dsi_rx_ctrl_dsc_async_handler
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.tp_heartbeat_exec) for tp_heartbeat_exec
    ap_demo.o(i.ap_demo) refers to app_tp_st_touch.o(i.app_tp_calibration_exec) for app_tp_calibration_exec
    ap_demo.o(i.ap_demo) refers to app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec) for ap_tp_st_touch_scan_point_record_event_exec
    ap_demo.o(i.ap_demo) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_transfer_screen_int) for app_tp_transfer_screen_int
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.S20_Start_init) for S20_Start_init
    ap_demo.o(i.ap_demo) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_demo) refers to app_tp_for_custom_s8.o(.data) for tp_sleep_count
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.soft_timer3_cb) for soft_timer3_cb
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.ap_reset_cb) for ap_reset_cb
    ap_demo.o(i.ap_get_reg_ca) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_get_reg_df) refers to ap_demo.o(i.blue_change_ccm) for blue_change_ccm
    ap_demo.o(i.ap_get_reg_df) refers to memcpya.o(.text) for __aeabi_memcpy4
    ap_demo.o(i.ap_get_reg_df) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) for hal_dsi_tx_ctrl_set_ccm
    ap_demo.o(i.ap_get_reg_df) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_reset_cb) refers to hal_system.o(i.hal_system_set_pvd) for hal_system_set_pvd
    ap_demo.o(i.ap_reset_cb) refers to hal_system.o(i.hal_system_set_vcc) for hal_system_set_vcc
    ap_demo.o(i.ap_set_backlight) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    ap_demo.o(i.ap_set_backlight) refers to idiv.o(.text) for __aeabi_idivmod
    ap_demo.o(i.ap_set_backlight) refers to uidiv.o(.text) for __aeabi_uidivmod
    ap_demo.o(i.ap_set_backlight) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_backlight) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_set_display_off) refers to ap_demo.o(i.Gpio_swire_output) for Gpio_swire_output
    ap_demo.o(i.ap_set_display_off) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_display_off) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_set_display_on) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to hal_timer.o(i.hal_timer_init) for hal_timer_init
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to ap_demo.o(i.disable_mipi_timer_cb) for disable_mipi_timer_cb
    ap_demo.o(i.ap_set_exit_sleep_mode) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_set_tp_calibration_04) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_update_frame_rate) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex) for hal_dsi_rx_ctrl_set_tear_mode_ex
    ap_demo.o(i.ap_update_frame_rate) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.blue_change_ccm) refers to memcpya.o(.text) for __aeabi_memcpy4
    ap_demo.o(i.blue_change_ccm) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) for hal_dsi_tx_ctrl_set_ccm
    ap_demo.o(i.disable_mipi_timer_cb) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    ap_demo.o(i.disable_mipi_timer_cb) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) for hal_dsi_tx_ctrl_stop
    ap_demo.o(i.disable_mipi_timer_cb) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) for hal_dsi_tx_ctrl_deinit
    ap_demo.o(i.disable_mipi_timer_cb) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) for hal_dsi_rx_ctrl_stop
    ap_demo.o(i.disable_mipi_timer_cb) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) for hal_dsi_rx_ctrl_deinit
    ap_demo.o(i.disable_mipi_timer_cb) refers to hal_swire.o(i.hal_swire_open) for hal_swire_open
    ap_demo.o(i.disable_mipi_timer_cb) refers to hal_timer.o(i.hal_timer_stop) for hal_timer_stop
    ap_demo.o(i.disable_mipi_timer_cb) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    ap_demo.o(i.disable_mipi_timer_cb) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin) for hal_dsi_tx_ctrl_panel_reset_pin
    ap_demo.o(i.disable_mipi_timer_cb) refers to hal_system.o(i.hal_system_set_vcc) for hal_system_set_vcc
    ap_demo.o(i.disable_mipi_timer_cb) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.disable_mipi_timer_cb) refers to app_tp_for_custom_s8.o(.data) for tp_sleep_in
    ap_demo.o(i.init_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) for hal_dsi_tx_ctrl_create_handle
    ap_demo.o(i.init_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    ap_demo.o(i.init_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) for hal_dsi_tx_ctrl_set_overwrite_rgb
    ap_demo.o(i.init_mipi_tx) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin) for hal_dsi_tx_ctrl_panel_reset_pin
    ap_demo.o(i.init_panel) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) for hal_dsi_tx_ctrl_enter_init_panel_mode
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) for hal_dsi_tx_ctrl_write_array_cmd
    ap_demo.o(i.init_panel) refers to tau_delay.o(i.delayUs) for delayUs
    ap_demo.o(i.init_panel) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    ap_demo.o(i.init_panel) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) for hal_dsi_rx_ctrl_set_hw_tear_mode
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) for hal_dsi_tx_ctrl_exit_init_panel_mode
    ap_demo.o(i.init_panel) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.open_mipi_rx) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) for hal_dsi_rx_ctrl_create_handle
    ap_demo.o(i.open_mipi_rx) refers to memcpya.o(.text) for __aeabi_memcpy4
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) for hal_dsi_rx_ctrl_pre_init_pps
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) for hal_dsi_rx_ctrl_set_cus_sync_line
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) for hal_dsi_rx_ctrl_hight_performan_mode
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(.constdata) for .constdata
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(i.ap_dcs_read) for ap_dcs_read
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(i.pps_update_handle) for pps_update_handle
    ap_demo.o(i.pps_update_handle) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) for hal_dsi_rx_ctrl_set_sw_tear_mode
    ap_demo.o(i.pps_update_handle) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) for hal_dsi_rx_ctrl_toggle_resolution
    ap_demo.o(i.pps_update_handle) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) for hal_dsi_rx_ctrl_set_hw_tear_mode
    ap_demo.o(i.pps_update_handle) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.soft_timer3_cb) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    ap_demo.o(i.soft_timer3_cb) refers to app_tp_for_custom_s8.o(.data) for tp_sleep_count
    ap_demo.o(i.soft_timer3_cb) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.tp_heartbeat_exec) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    ap_demo.o(i.tp_heartbeat_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) for ap_tp_st_touch_software_reset
    ap_demo.o(i.tp_heartbeat_exec) refers to app_tp_transfer.o(.data) for s_screen_init_complate
    ap_demo.o(i.tp_heartbeat_exec) refers to ap_demo.o(.data) for .data
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_display_on) for ap_set_display_on
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_display_off) for ap_set_display_off
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_get_reg_df) for ap_get_reg_df
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_get_reg_ca) for ap_get_reg_ca
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_backlight) for ap_set_backlight
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_update_frame_rate) for ap_update_frame_rate
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_enter_sleep_mode) for ap_set_enter_sleep_mode
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_exit_sleep_mode) for ap_set_exit_sleep_mode
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_tp_calibration_04) for ap_set_tp_calibration_04
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_transfer.o(i.S20_Start_init) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.S20_Start_init) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_ctrl_eint) for hal_gpio_ctrl_eint
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_init_eint) for hal_gpio_init_eint
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_reg_eint_cb) for hal_gpio_reg_eint_cb
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_for_custom_s8.o(.data) for screen_reg_int_data
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(i.app_tp_screen_int_callback) for app_tp_screen_int_callback
    app_tp_transfer.o(i.S20_Start_init) refers to ap_demo.o(.data) for phone_start_flag
    app_tp_transfer.o(i.app_tp_I2C_init) refers to hal_i2c_slave.o(i.hal_i2c_s_init) for hal_i2c_s_init
    app_tp_transfer.o(i.app_tp_I2C_init) refers to hal_i2c_slave.o(i.hal_i2c_s_set_transfer) for hal_i2c_s_set_transfer
    app_tp_transfer.o(i.app_tp_I2C_init) refers to hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read) for hal_i2c_s_nonblocking_read
    app_tp_transfer.o(i.app_tp_I2C_init) refers to app_tp_transfer.o(i.app_tp_i2cs_callback) for app_tp_i2cs_callback
    app_tp_transfer.o(i.app_tp_I2C_init) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) for app_tp_phone_analysis_data
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(i.app_tp_s_read) for app_tp_s_read
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(i.app_tp_s_write) for app_tp_s_write
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.app_tp_init) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(i.app_tp_screen_init) for app_tp_screen_init
    app_tp_transfer.o(i.app_tp_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    app_tp_transfer.o(i.app_tp_init) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_master.o(i.hal_i2c_m_dma_init) for hal_i2c_m_dma_init
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_for_custom_s8.o(.data) for g_phone_output_int_pad
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.app_tp_m_read) refers to hal_i2c_master.o(i.hal_i2c_m_dma_read) for hal_i2c_m_dma_read
    app_tp_transfer.o(i.app_tp_m_transfer_complate) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.app_tp_m_write) refers to hal_i2c_master.o(i.hal_i2c_m_dma_write) for hal_i2c_m_dma_write
    app_tp_transfer.o(i.app_tp_phone_clear_reset_on) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_phone_reset_on) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_s_read) refers to hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read) for hal_i2c_s_nonblocking_read
    app_tp_transfer.o(i.app_tp_s_transfer_complate) refers to hal_i2c_slave.o(i.hal_i2c_s_write_complate) for hal_i2c_s_write_complate
    app_tp_transfer.o(i.app_tp_s_transfer_complate) refers to hal_i2c_slave.o(i.hal_i2c_s_read_complate) for hal_i2c_s_read_complate
    app_tp_transfer.o(i.app_tp_s_write) refers to hal_i2c_slave.o(i.hal_i2c_s_dma_write) for hal_i2c_s_dma_write
    app_tp_transfer.o(i.app_tp_screen_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    app_tp_transfer.o(i.app_tp_screen_init) refers to tau_delay.o(i.delayUs) for delayUs
    app_tp_transfer.o(i.app_tp_screen_init) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_transfer.o(i.app_tp_screen_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_rst_pad
    app_tp_transfer.o(i.app_tp_screen_int_callback) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to hal_spi_master.o(i.hal_spi_m_clear_rxfifo) for hal_spi_m_clear_rxfifo
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(i.S20_Start_init) for S20_Start_init
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_for_custom_s8.o(.constdata) for screen_reg_start_data_size
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to ap_demo.o(.data) for phone_start_flag
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_spi_master.o(i.hal_spi_m_clear_rxfifo) for hal_spi_m_clear_rxfifo
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to tau_delay.o(i.delayUs) for delayUs
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_transfer_screen_const) for app_tp_transfer_screen_const
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event) for ap_tp_st_touch_scan_point_record_event
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_FF) for ap_tp_st_touch_error_handler_FF
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_F3) for ap_tp_st_touch_error_handler_F3
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) for app_tp_screen_analysis_int
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(.data) for screen_reg_int_data
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.app_tp_transfer_screen_start) refers to app_tp_transfer.o(i.app_tp_transfer_screen_const) for app_tp_transfer_screen_const
    app_tp_transfer.o(i.app_tp_transfer_screen_start) refers to app_tp_transfer.o(.data) for .data
    app_tp_st_touch.o(i.CRC16_2) refers to app_tp_st_touch.o(.constdata) for .constdata
    app_tp_st_touch.o(i.ap_get_tp_calibration_status_01) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) for hal_dsi_rx_ctrl_send_ack_cmd
    app_tp_st_touch.o(i.ap_get_tp_calibration_status_01) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.ap_set_tp_calibration_04) refers to memseta.o(.text) for __aeabi_memclr4
    app_tp_st_touch.o(i.ap_set_tp_calibration_04) refers to printfa.o(i.__0printf) for __2printf
    app_tp_st_touch.o(i.ap_set_tp_calibration_04) refers to app_tp_st_touch.o(i.CRC16_2) for CRC16_2
    app_tp_st_touch.o(i.ap_set_tp_calibration_04) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.ap_tp_st_touch_calibration) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_st_touch.o(i.ap_tp_st_touch_calibration) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_st_touch.o(i.ap_tp_st_touch_calibration) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_calibration) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_F3) refers to app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) for ap_tp_st_touch_software_reset
    app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_FF) refers to app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) for ap_tp_st_touch_software_reset
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to memseta.o(.text) for __aeabi_memclr4
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event) for ap_tp_st_touch_simulate_finger_release_event
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init) for ap_tp_st_touch_scan_point_init
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_rst_pad
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init) refers to app_tp_st_touch.o(.bss) for .bss
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event) refers to app_tp_st_touch.o(.bss) for .bss
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event) for ap_tp_st_touch_simulate_finger_release_event
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init) for ap_tp_st_touch_scan_point_init
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec) refers to app_tp_st_touch.o(.bss) for .bss
    app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event) refers to app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) for app_tp_screen_analysis_int
    app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event) for ap_tp_st_touch_simulate_finger_release_event
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init) for ap_tp_st_touch_scan_point_init
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_calibration) for ap_tp_st_touch_calibration
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) for ap_tp_st_touch_get_calibration_success_mark
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to app_tp_st_touch.o(.data) for .data
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_init) for hal_system_init
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_enable_systick) for hal_system_enable_systick
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_init_console) for hal_system_init_console
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_set_phy_calibration) for hal_system_set_phy_calibration
    startup_armcm0.o(RESET) refers to startup_armcm0.o(STACK) for __initial_sp
    startup_armcm0.o(RESET) refers to startup_armcm0.o(.text) for Reset_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.HardFault_Handler) for HardFault_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SysTick_Handler) for SysTick_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.VIDC_IRQn_Handler) for VIDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.LCDC_IRQn_Handler) for LCDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.MIPI_RX_IRQn_Handler) for MIPI_RX_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.MIPI_TX_IRQn_Handler) for MIPI_TX_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.MEMC_IRQn_Handler) for MEMC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.VPRE_IRQn_Handler) for VPRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.FLSCTRL_IRQn_Handler) for FLSCTRL_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.DMA_IRQn_Handler) for DMA_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER0_IRQn_Handler) for TIMER0_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER1_IRQn_Handler) for TIMER1_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER2_IRQn_Handler) for TIMER2_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER3_IRQn_Handler) for TIMER3_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.WDG_IRQn_Handler) for WDG_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.UART_IRQn_Handler) for UART_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.I2C0_IRQn_Handler) for I2C0_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.I2C1_IRQn_Handler) for I2C1_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SPIS_IRQn_Handler) for SPIS_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SPIM_IRQn_Handler) for SPIM_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.ADC_IRQn_Handler) for ADC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.PWMDET_IRQn_Handler) for PWMDET_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SWIRE_IRQn_Handler) for SWIRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.AP_NRESET_IRQn_Handler) for AP_NRESET_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT0_IRQn_Handler) for EXTI_INT0_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT1_IRQn_Handler) for EXTI_INT1_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT2_IRQn_Handler) for EXTI_INT2_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT3_IRQn_Handler) for EXTI_INT3_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT4_IRQn_Handler) for EXTI_INT4_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT5_IRQn_Handler) for EXTI_INT5_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT6_IRQn_Handler) for EXTI_INT6_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT7_IRQn_Handler) for EXTI_INT7_IRQn_Handler
    startup_armcm0.o(.text) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to drv_vidc.o(i.drv_vidc_set_module_enable) for drv_vidc_set_module_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) for hal_internal_vsync_get_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) for dcs_packet_get_fifo_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) for dcs_packet_free_fifo_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg) for drv_dsi_rx_set_ddi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_crgu.o(i.drv_crgu_set_rxbr_src) for drv_crgu_set_rxbr_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_crgu.o(i.drv_crgu_set_rxbr_div) for drv_crgu_set_rxbr_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg) for drv_dsi_rx_set_ipi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_gen_a_tear_signal) for drv_memc_gen_a_tear_signal
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size) for drv_dsi_rx_get_max_ret_size
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) for hal_dsi_rx_ctrl_init_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_rx) for hal_internal_vsync_init_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) for hal_dsi_rx_ctrl_init_dsi_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) for hal_dsi_rx_ctrl_init_rxbr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps) for drv_dsc_dec_set_u8_pps
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) for hal_dsi_rx_ctrl_init_vidc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) for hal_dsi_rx_ctrl_init_memc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_chip_info.o(i.drv_chip_rx_init_done) for drv_chip_rx_init_done
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_vidc_src) for drv_crgu_set_vidc_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_fb_src) for drv_crgu_set_fb_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_fb_div) for drv_crgu_set_fb_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) for hal_dsi_rx_ctrl_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg) for drv_dsi_rx_set_ctrl_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) for drv_dsi_rx_set_up_phy
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap) for drv_dsi_rx_set_lane_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_inten) for drv_dsi_rx_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt) for drv_dsi_rx_set_resp_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_mode) for drv_memc_set_ltpo_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tear_mode) for hal_internal_vsync_get_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_fs_en_conditions) for drv_memc_set_fs_en_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_lcdc_st_conditions) for drv_memc_set_lcdc_st_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_vidc_sync_cnt) for drv_memc_set_vidc_sync_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_double_buffer) for drv_memc_set_double_buffer
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_active_height) for drv_memc_set_active_height
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_inten) for drv_memc_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_color_format) for drv_rxbr_set_color_format
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th) for drv_rxbr_set_ltpo_drop_th
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_cfg) for drv_rxbr_set_usr_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_col) for drv_rxbr_set_usr_col
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_row) for drv_rxbr_set_usr_row
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg) for drv_rxbr_hline_rcv_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) for hal_internal_vsync_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_src_parameter) for drv_vidc_set_src_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pentile_swap) for drv_vidc_set_pentile_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_dst_parameter) for drv_vidc_set_dst_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_init_module_enable) for drv_vidc_init_module_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_rotation) for drv_vidc_set_rotation
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_init_get_scld_filter_h) for drv_param_init_get_scld_filter_h
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_init_get_scld_filter_v) for drv_param_init_get_scld_filter_v
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef0) for drv_vidc_set_scld_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef1) for drv_vidc_set_scld_hcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef0) for drv_vidc_set_scld_vcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef1) for drv_vidc_set_scld_vcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_p2r_hinitr) for drv_vidc_set_p2r_hinitr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_p2r_hinitb) for drv_vidc_set_p2r_hinitb
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_p2r_filter_init) for drv_param_p2r_filter_init
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_p2r_hcoef0) for drv_vidc_set_p2r_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_mirror) for drv_vidc_set_mirror
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pu_ctrl) for drv_vidc_set_pu_ctrl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter) for drv_dsc_dec_convert_pps_rc_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header) for drv_rxbr_set_ack_pkt_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) for hal_internal_vsync_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef0) for drv_vidc_set_scld_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef1) for drv_vidc_set_scld_hcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef0) for drv_vidc_set_scld_vcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef1) for drv_vidc_set_scld_vcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_param_init.o(i.drv_param_init_set_scld_filter) for drv_param_init_set_scld_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) for hal_internal_vsync_set_sync_line
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg) for drv_rxbr_hline_rcv0_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_dcs_direct_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode) for hal_internal_vsync_set_dcs_direct_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) refers to drv_rxbr.o(i.drv_rxbr_set_cmd_filter) for drv_rxbr_set_cmd_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) for drv_dsi_rx_calc_ipi_tx_delay
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg) for drv_dsi_rx_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format) refers to drv_vidc.o(i.drv_vidc_update_src_format) for drv_vidc_update_src_format
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format) refers to drv_vidc.o(i.drv_vidc_set_pentile_swap) for drv_vidc_set_pentile_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dflti.o(.text) for __aeabi_i2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dmul.o(.text) for __aeabi_dmul
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to ddiv.o(.text) for __aeabi_ddiv
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to dflti.o(.text) for __aeabi_i2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to dmul.o(.text) for __aeabi_dmul
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to ddiv.o(.text) for __aeabi_ddiv
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) for hal_dsi_rx_ctrl_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_src) for drv_crgu_set_rxbr_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_div) for drv_crgu_set_rxbr_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_dsco_src) for drv_crgu_set_dsco_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_dsco_src_div) for drv_crgu_set_dsco_src_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_dsc_core_div) for drv_crgu_set_dsc_core_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_te_waveform) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_te_waveform) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_dsi_rx.o(i.drv_dsi_rx_power_up) for drv_dsi_rx_power_up
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) for hal_internal_vsync_toggle_input_frame_rate
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) for hal_internal_sync_input_resolution_change
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution_ex) refers to hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) for hal_internal_sync_input_resolution_change_ex
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution_ex) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_register_write_cmd_entry) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) for hal_dsi_rx_ctrl_set_hw_cmd_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_register_write_cmd_entry) refers to hal_internal_vsync.o(i.hal_internal_vsync_register_write_cmd_entry) for hal_internal_vsync_register_write_cmd_entry
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fscalb.o(.text) for __ARM_scalbnf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fflti.o(.text) for __aeabi_i2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to ffixi.o(.text) for __aeabi_f2iz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk) for drv_dsi_tx_set_video_chunk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing) for drv_dsi_tx_set_video_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to drv_phy_common.o(i.drv_phy_get_rate_para) for drv_phy_get_rate_para
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to ffixui.o(.text) for __aeabi_f2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to hal_dsi_tx_ctrl.o(.conststring) for .conststring
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) for hal_lcdc_config_upscaler
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to drv_lcdc.o(i.drv_lcdc_config_src_parameter) for drv_lcdc_config_src_parameter
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to hal_internal_vsync.o(i.hal_internal_vsync_update_lcdc_addr) for hal_internal_vsync_update_lcdc_addr
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode_rcv_te) refers to hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) for hal_internal_sync_cmd_mode_rcv_te
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_param_init.o(i.drv_param_init_set_ccm) for drv_param_init_set_ccm
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.constdata) for .constdata
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) for hal_lcdc_config_upscaler
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) for hal_lcdc_config_remains
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_mode_init) for hal_dsi_tx_ctrl_draw_mode_init
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) for hal_dsi_tx_ctrl_set_rect_pixel_data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) for hal_lcdc_config_upscaler
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) for hal_lcdc_config_remains
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_mode_init) for hal_dsi_tx_ctrl_draw_mode_init
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_ulps_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) for drv_dsi_tx_phy_ulps_enter
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_ulps_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) for drv_dsi_tx_phy_ulps_exit
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) for hal_dsi_tx_ctrl_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_tx) for hal_internal_vsync_init_tx
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate) for hal_dsi_tx_config_params_for_lane_rate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) for hal_dsi_tx_count_lane_rate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) for hal_dsi_tx_init_phy_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) for drv_dsi_tx_phy_test_setup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) for hal_lcdc_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) for hal_lcdc_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) for hal_dsi_tx_init_dpi_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) for hal_dsi_tx_init_data_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) for hal_dsi_tx_init_remains
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt) for hal_dsi_tx_init_interrupt
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready) for drv_dsi_tx_phy_status_ready
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload) for drv_dsi_tx_command_get_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) refers to drv_param_init.o(i.drv_param_init_set_ccm) for drv_param_init_set_ccm
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_pq_filter) refers to drv_lcdc.o(i.drv_lcdc_config_scale_up_coef) for drv_lcdc_config_scale_up_coef
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_pq_filter) refers to drv_param_init.o(i.drv_param_init_set_sclu_filter) for drv_param_init_set_sclu_filter
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness) refers to drv_lcdc.o(i.drv_lcdc_config_endianness) for drv_lcdc_config_endianness
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_lp_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd) for drv_dsi_tx_video_mode_set_lp_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb) for drv_lcdc_config_overwrite_rgb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp) refers to drv_lcdc.o(i.drv_lcdc_config_partial_display_enable) for drv_lcdc_config_partial_display_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area) refers to drv_lcdc.o(i.drv_lcdc_config_partial_display_area) for drv_lcdc_config_partial_display_area
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to dflti.o(.text) for __aeabi_i2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to dmul.o(.text) for __aeabi_dmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to ddiv.o(.text) for __aeabi_ddiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_vpg) for drv_dsi_tx_set_vpg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) for hal_dsi_tx_ctrl_draw_flicker
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) for hal_dsi_tx_ctrl_draw_chessboard
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_enable_shadow_reg) for drv_lcdc_enable_shadow_reg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_set_video_hw_mode) for drv_lcdc_set_video_hw_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_start) for drv_lcdc_start
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size) for drv_dsi_tx_edpi_cmd_size
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) for hal_dsi_tx_init_video_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode) for drv_dsi_tx_dpi_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity) for drv_dsi_tx_dpi_polarity
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time) for drv_dsi_tx_dpi_lpcmd_time
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_int) for drv_dsi_tx_config_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode) for drv_dsi_tx_phy_lane_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg) for drv_dsi_tx_phy_time_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_response_mode) for drv_dsi_tx_response_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div) for drv_dsi_tx_set_time_out_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg) for drv_dsi_tx_timeout_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp) for drv_dsi_tx_phy_clock_lane_auto_lp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg) for drv_dsi_tx_video_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack) for drv_dsi_tx_set_bta_ack
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd) for drv_dsi_tx_video_mode_set_lp_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_disable_hact_cmd) for drv_dsi_tx_video_mode_disable_hact_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) for hal_dsi_tx_calc_video_chunks
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_header) for drv_dsi_tx_command_header
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) refers to drv_param_init.o(i.drv_param_init_get_ccm) for drv_param_init_get_ccm
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) refers to drv_lcdc.o(i.drv_lcdc_config_ccm) for drv_lcdc_config_ccm
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_disp_mode) for drv_lcdc_config_disp_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_edpi_mode) for drv_lcdc_config_edpi_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_endianness) for drv_lcdc_config_endianness
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_thresh) for drv_lcdc_config_thresh
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_dpi_polarity) for drv_lcdc_config_dpi_polarity
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_src_parameter) for drv_lcdc_config_src_parameter
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area) for hal_dsi_tx_ctrl_set_partial_disp_area
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp) for hal_dsi_tx_ctrl_set_partial_disp
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_lcdc.o(i.drv_lcdc_config_scale_up_step) for drv_lcdc_config_scale_up_step
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_param_init.o(i.drv_param_init_get_sclu_filter) for drv_param_init_get_sclu_filter
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_lcdc.o(i.drv_lcdc_config_scale_up_coef) for drv_lcdc_config_scale_up_coef
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) for hal_lcdc_config_upscaler
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) for hal_lcdc_config_ccm
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile) for hal_lcdc_config_rgb_to_pentile
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) for hal_lcdc_config_remains
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) for hal_lcdc_init_interrupt
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to drv_lcdc.o(i.drv_lcdc_set_prefetch) for drv_lcdc_set_prefetch
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dpi_pre_div) for drv_crgu_set_dpi_pre_div
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dpi_pre_src) for drv_crgu_set_dpi_pre_src
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dpi_mux_src) for drv_crgu_set_dpi_mux_src
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_lcdc.o(i.drv_lcdc_config_dpi_timing) for drv_lcdc_config_dpi_timing
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to hal_internal_vsync.o(i.hal_internal_update_dpi_param) for hal_internal_update_dpi_param
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to cfrcmple.o(.text) for __aeabi_cfrcmple
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ffixi.o(.text) for __aeabi_f2iz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_lcdc_div) for drv_crgu_set_lcdc_div
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_lcdc_src) for drv_crgu_set_lcdc_src
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to drv_lcdc.o(i.drv_lcdc_ctrl_flow) for drv_lcdc_ctrl_flow
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to drv_lcdc.o(i.drv_lcdc_config_int) for drv_lcdc_config_int
    hal_gpio.o(i.hal_gpio_ctrl_eint) refers to drv_gpio.o(i.drv_gpio_set_int) for drv_gpio_set_int
    hal_gpio.o(i.hal_gpio_ctrl_eint) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_get_input_data) refers to drv_gpio.o(i.drv_gpio_get_input_data) for drv_gpio_get_input_data
    hal_gpio.o(i.hal_gpio_get_int_type) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to drv_gpio.o(i.drv_gpio_get_pull_state) for drv_gpio_get_pull_state
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_eint) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group) for drv_sys_cfg_sel_gpio_group
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig) for drv_sys_cfg_sel_int_trig
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_init_eint) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_input) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_input) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_input) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_init_output) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_reg_eint_cb) refers to drv_gpio.o(i.drv_gpio_register_callback) for drv_gpio_register_callback
    hal_gpio.o(i.hal_gpio_reg_eint_cb) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_gpio.o(i.drv_gpio_register_ap_reset_callback) for drv_gpio_register_ap_reset_callback
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) for drv_sys_cfg_sel_ap_rst_trig
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to drv_gpio.o(i.drv_gpio_set_driving_strength) for drv_gpio_set_driving_strength
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode3) for drv_gpio_set_mode3
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode2) for drv_gpio_set_mode2
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode1) for drv_gpio_set_mode1
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode0) for drv_gpio_set_mode0
    hal_gpio.o(i.hal_gpio_set_mode) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_output_data) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to drv_gpio.o(i.drv_gpio_set_pull_state) for drv_gpio_set_pull_state
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to drv_gpio.o(i.drv_gpio_set_schmitt_trigger) for drv_gpio_set_schmitt_trigger
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to drv_gpio.o(i.drv_gpio_set_slew_rate) for drv_gpio_set_slew_rate
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to hal_gpio.o(.constdata) for .constdata
    hal_i2c_master.o(i.hal_i2c_m_deinit) refers to drv_i2c_master.o(i.drv_i2c_m_deinit) for drv_i2c_m_deinit
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_master.o(i.drv_i2c_master_init) for drv_i2c_master_init
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_master.o(i.drv_i2c1_set_callback) for drv_i2c1_set_callback
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_master.o(i.drv_i2c_m_enable_intr) for drv_i2c_m_enable_intr
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_dma.o(i.drv_i2c_dma_init) for drv_i2c_dma_init
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_dma.o(i.drv_i2c_enable_rx_dma) for drv_i2c_enable_rx_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_dma.o(i.drv_i2c_enable_tx_dma) for drv_i2c_enable_tx_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to hal_i2c_master.o(i.hal_i2c_master_irq_callback) for hal_i2c_master_irq_callback
    hal_i2c_master.o(i.hal_i2c_m_dma_read) refers to drv_i2c_dma.o(i.drv_i2c_master_read_dma) for drv_i2c_master_read_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_read) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_master.o(i.hal_i2c_m_dma_write) refers to drv_i2c_dma.o(i.drv_i2c_master_write_dma) for drv_i2c_master_write_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_write) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_master.o(i.hal_i2c_m_set_high_impedance) refers to drv_i2c_master.o(i.drv_i2c_m_enable) for drv_i2c_m_enable
    hal_i2c_master.o(i.hal_i2c_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_master.o(i.hal_i2c_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_i2c_master.o(i.hal_i2c_m_transfer_complate) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_master.o(i.hal_i2c_master_irq_callback) refers to drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit) for drv_i2c_m_clear_it_pending_bit
    hal_i2c_master.o(i.hal_i2c_master_irq_callback) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to drv_i2c_slave.o(i.drv_i2c_s_set_intr) for drv_i2c_s_set_intr
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to drv_i2c_slave.o(i.drv_i2c_s_enable) for drv_i2c_s_enable
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to drv_i2c_dma.o(i.drv_i2c_slave_write_dma) for drv_i2c_slave_write_dma
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_get_tx_byte_num) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c_slave_init) for drv_i2c_slave_init
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_master.o(i.drv_i2c1_set_callback) for drv_i2c1_set_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c_s_config_intr) for drv_i2c_s_config_intr
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c_s_set_intr) for drv_i2c_s_set_intr
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_dma.o(i.drv_i2c_dma_init) for drv_i2c_dma_init
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) for drv_i2c_set_dma_irq_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_dma.o(i.drv_i2c_enable_tx_dma) for drv_i2c_enable_tx_dma
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c0_set_callback) for drv_i2c0_set_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) for hal_i2c_slave_irq_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback) for hal_i2c_s_dma_user_callback
    hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_complate) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_complate_clear) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_data) refers to drv_i2c_slave.o(i.drv_i2c_s_read_data) for drv_i2c_s_read_data
    hal_i2c_slave.o(i.hal_i2c_s_read_data) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_data) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_rxfifo_notempty) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    hal_i2c_slave.o(i.hal_i2c_s_rxfifo_notempty) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_rxfifo_notempty) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_sel) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_set_dma_tx_cycle) refers to drv_dma.o(i.drv_dma_enable_cycle) for drv_dma_enable_cycle
    hal_i2c_slave.o(i.hal_i2c_s_set_dma_tx_cycle) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_set_dma_tx_cycle) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to drv_i2c_slave.o(i.drv_i2c_s_enable) for drv_i2c_s_enable
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_set_transfer) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_write_complate) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_write_data) refers to drv_i2c_slave.o(i.drv_i2c_s_write_data) for drv_i2c_s_write_data
    hal_i2c_slave.o(i.hal_i2c_s_write_data) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_write_data) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit) for drv_i2c_s_clear_it_pending_bit
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(i.drv_i2c_s_write_data) for drv_i2c_s_write_data
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_spi_master.o(i.hal_spi_m_callback) refers to drv_spi_dma.o(i.drv_spi_abort_dma) for drv_spi_abort_dma
    hal_spi_master.o(i.hal_spi_m_callback) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_clear_rxfifo) refers to drv_spi_master.o(i.drv_spi_m_read_data) for drv_spi_m_read_data
    hal_spi_master.o(i.hal_spi_m_deinit) refers to drv_spi_master.o(i.drv_spi_m_deinit) for drv_spi_m_deinit
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to hal_spi_master.o(i.hal_spi_m_gpio_init) for hal_spi_m_gpio_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_master.o(i.drv_spi_master_init) for drv_spi_master_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_dma_init) for drv_spi_dma_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_dma_ch6_init) for drv_spi_dma_ch6_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) for drv_spi_set_dma_irq_callback
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) for drv_spi_set_dma_ch6_irq_callback
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req) for drv_sys_cfg_set_dma_rx_req
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_master.o(i.drv_spi_m_enable_rx_dma) for drv_spi_m_enable_rx_dma
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to hal_spi_master.o(i.hal_spi_m_callback) for hal_spi_m_callback
    hal_spi_master.o(i.hal_spi_m_dma_read) refers to drv_spi_dma.o(i.drv_spim_dma_read) for drv_spim_dma_read
    hal_spi_master.o(i.hal_spi_m_dma_read) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_dma_write) refers to drv_spi_dma.o(i.drv_spim_dma_write) for drv_spim_dma_write
    hal_spi_master.o(i.hal_spi_m_dma_write) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_get_transfer_complate) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_gpio_init) refers to drv_spi_master.o(i.drv_spi_m_gpio_init) for drv_spi_m_gpio_init
    hal_spi_master.o(i.hal_spi_m_read_rxfifo) refers to drv_spi_master.o(i.drv_spi_m_read_data) for drv_spi_m_read_data
    hal_spi_master.o(i.hal_spi_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_spi_master.o(i.hal_spi_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    hal_spi_master.o(i.hal_spi_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_swire.o(i.hal_swire_deinit) refers to drv_swire.o(i.drv_swire_enable) for drv_swire_enable
    hal_swire.o(i.hal_swire_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_swire.o(i.hal_swire_init) refers to drv_crgu.o(i.drv_crgu_set_swire_div) for drv_crgu_set_swire_div
    hal_swire.o(i.hal_swire_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_swire.o(i.hal_swire_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_swire.o(i.hal_swire_init) refers to drv_swire.o(i.drv_swire_enable) for drv_swire_enable
    hal_swire.o(i.hal_swire_open) refers to drv_swire.o(i.drv_swire_set_power_down) for drv_swire_set_power_down
    hal_swire.o(i.hal_swire_register_callback) refers to drv_swire.o(i.drv_swire_register_callback) for drv_swire_register_callback
    hal_swire.o(i.hal_swire_start) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    hal_swire.o(i.hal_swire_start) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_swire.o(i.hal_swire_start) refers to drv_swire.o(i.drv_swire_set_bit_time) for drv_swire_set_bit_time
    hal_swire.o(i.hal_swire_start) refers to drv_swire.o(i.drv_swire_set_pulse_count) for drv_swire_set_pulse_count
    hal_swire.o(i.hal_swire_start) refers to drv_common.o(.data) for g_system_clock
    hal_system.o(i.hal_system_deep_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode) for drv_pwr_enter_deep_sleep_mode
    hal_system.o(i.hal_system_disable_systick) refers to drv_common.o(i.drv_common_disable_systick) for drv_common_disable_systick
    hal_system.o(i.hal_system_enable_systick) refers to drv_common.o(i.drv_common_enable_systick) for drv_common_enable_systick
    hal_system.o(i.hal_system_get_tick) refers to drv_common.o(i.drv_common_get_tick) for drv_common_get_tick
    hal_system.o(i.hal_system_idle_mode) refers to drv_common.o(i.drv_common_idle_mode) for drv_common_idle_mode
    hal_system.o(i.hal_system_init) refers to drv_pwr.o(i.drv_pwr_set_system_clk_src) for drv_pwr_set_system_clk_src
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_set_ahb_src) for drv_crgu_set_ahb_src
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_set_ahb_pre_div) for drv_crgu_set_ahb_pre_div
    hal_system.o(i.hal_system_init) refers to irq_redirect .o(i.handle_init) for handle_init
    hal_system.o(i.hal_system_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int) for drv_sys_cfg_clear_all_int
    hal_system.o(i.hal_system_init) refers to drv_common.o(i.drv_common_system_init) for drv_common_system_init
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_system.o(i.hal_system_init) refers to drv_pwr.o(i.drv_pwr_set_pvd_mode) for drv_pwr_set_pvd_mode
    hal_system.o(i.hal_system_init) refers to drv_common.o(.data) for g_system_clock
    hal_system.o(i.hal_system_init_console) refers to hal_uart.o(i.hal_uart_init) for hal_uart_init
    hal_system.o(i.hal_system_register_systick_cb) refers to drv_common.o(i.drv_common_systick_register_cb) for drv_common_systick_register_cb
    hal_system.o(i.hal_system_set_phy_calibration) refers to drv_phy_common.o(i.drv_phy_enable_calibration) for drv_phy_enable_calibration
    hal_system.o(i.hal_system_set_pvd) refers to drv_pwr.o(i.drv_pwr_set_pvd_mode) for drv_pwr_set_pvd_mode
    hal_system.o(i.hal_system_set_vcc) refers to drv_pwr.o(i.drv_pwr_set_cp_mode) for drv_pwr_set_cp_mode
    hal_system.o(i.hal_system_share_flash_mode) refers to drv_fls.o(i.drv_fls_gpio_connect) for drv_fls_gpio_connect
    hal_system.o(i.hal_system_share_flash_mode) refers to drv_fls.o(i.drv_fls_gpio_disconnect) for drv_fls_gpio_disconnect
    hal_system.o(i.hal_system_sleep_mode) refers to drv_crgu.o(i.drv_crgu_config_clocks) for drv_crgu_config_clocks
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_set_repeat) for drv_timer_set_repeat
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_timer.o(i.hal_timer_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_timer.o(i.hal_timer_get_status) refers to drv_timer.o(i.drv_timer_get_status) for drv_timer_get_status
    hal_timer.o(i.hal_timer_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_timer.o(i.hal_timer_init) refers to drv_timer.o(i.drv_timer_set_prescaler) for drv_timer_set_prescaler
    hal_timer.o(i.hal_timer_set_repeat) refers to drv_timer.o(i.drv_timer_set_repeat) for drv_timer_set_repeat
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_get_prescaler) for drv_timer_get_prescaler
    hal_timer.o(i.hal_timer_start) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_start) refers to drv_common.o(.data) for g_system_clock
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_get_prescaler) for drv_timer_get_prescaler
    hal_timer.o(i.hal_timer_start_ex) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_start_ex) refers to drv_common.o(.data) for g_system_clock
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    tau_delay.o(i.delayMs) refers to tau_delay.o(i.delayUs) for delayUs
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to app_tp_for_custom_s8.o(.data) for .data
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to app_tp_for_custom_s8.o(.constdata) for .constdata
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to app_tp_transfer.o(i.app_tp_screen_init) for app_tp_screen_init
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to app_tp_for_custom_s8.o(.data) for .data
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to app_tp_enc.o(i.EncryptCheck) for EncryptCheck
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to uidiv.o(.text) for __aeabi_uidivmod
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to app_tp_for_custom_s8.o(.data) for .data
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_1
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_2
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_3
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_4
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_5
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_6
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_7
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_point_data
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_point_back
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_coord_data
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_coord_back
    hal_uart.o(i.hal_uart_deinit) refers to drv_dma.o(i.drv_dma_deinit) for drv_dma_deinit
    hal_uart.o(i.hal_uart_deinit) refers to drv_uart.o(i.UART_Deinit) for UART_Deinit
    hal_uart.o(i.hal_uart_dmacallback) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_uart.o(i.hal_uart_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_uart.o(i.hal_uart_init) refers to drv_uart.o(i.UART_init) for UART_init
    hal_uart.o(i.hal_uart_init) refers to drv_common.o(.data) for g_system_clock
    hal_uart.o(i.hal_uart_init) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_receive_blocking) refers to drv_uart.o(i.UART_ReadBlocking) for UART_ReadBlocking
    hal_uart.o(i.hal_uart_receive_dma) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    hal_uart.o(i.hal_uart_receive_dma) refers to drv_uart_dma.o(i.UART_TransferCreateHandleDMA) for UART_TransferCreateHandleDMA
    hal_uart.o(i.hal_uart_receive_dma) refers to drv_uart_dma.o(i.UART_TransferReceiveDMA) for UART_TransferReceiveDMA
    hal_uart.o(i.hal_uart_receive_dma) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_receive_dma) refers to hal_uart.o(i.hal_uart_dmacallback) for hal_uart_dmacallback
    hal_uart.o(i.hal_uart_transmit_blocking) refers to drv_uart.o(i.UART_WriteBlocking) for UART_WriteBlocking
    hal_uart.o(i.hal_uart_transmit_dma) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    hal_uart.o(i.hal_uart_transmit_dma) refers to drv_uart_dma.o(i.UART_TransferCreateHandleDMA) for UART_TransferCreateHandleDMA
    hal_uart.o(i.hal_uart_transmit_dma) refers to drv_uart_dma.o(i.UART_TransferSendDMA) for UART_TransferSendDMA
    hal_uart.o(i.hal_uart_transmit_dma) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_transmit_dma) refers to hal_uart.o(i.hal_uart_dmacallback) for hal_uart_dmacallback
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_param_init.o(i.drv_param_init_get_ccm) for drv_param_init_get_ccm
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_lcdc.o(i.drv_lcdc_config_ccm) for drv_lcdc_config_ccm
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to f2d.o(.text) for __aeabi_f2d
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to ddiv.o(.text) for __aeabi_ddiv
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to sqrt.o(i.sqrt) for sqrt
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to dmul.o(.text) for __aeabi_dmul
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to cdcmple.o(.text) for __aeabi_cdcmple
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to hal_internal_vsync.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.dcs_sw_filter) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.dcs_sw_filter) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tear_mode) for hal_internal_vsync_get_tear_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_mode) for drv_memc_set_ltpo_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_double_buffer) for drv_memc_set_double_buffer
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_active_height) for drv_memc_set_active_height
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_inten) for drv_memc_set_inten
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) refers to drv_lcdc.o(i.drv_lcdc_start) for drv_lcdc_start
    hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) for hal_dsi_rx_ctrl_gen_a_tear_signal
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_delay.o(i.delayUs) for delayUs
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.hal_internal_init_memc) for hal_internal_init_memc
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to drv_lcdc.o(i.drv_lcdc_enable_shadow_reg) for drv_lcdc_enable_shadow_reg
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to tau_delay.o(i.delayMs) for delayMs
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) for hal_dsi_rx_ctrl_gen_a_tear_signal
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to tau_delay.o(i.delayUs) for delayUs
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) for hal_vsync_reset_lcdc_scaler
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_internal_vsync.o(i.vsync_set_te_mode) for vsync_set_te_mode
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.hal_internal_update_dpi_param) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_video_mode_auto_sync) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_internal_vsync.o(i.hal_internal_video_mode_auto_sync) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_vsync.o(i.hal_internal_video_mode_auto_sync) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_vsync.o(i.hal_internal_video_mode_auto_sync) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_vsync.o(i.hal_internal_video_mode_auto_sync) refers to f2d.o(.text) for __aeabi_f2d
    hal_internal_vsync.o(i.hal_internal_video_mode_auto_sync) refers to dadd.o(.text) for __aeabi_dadd
    hal_internal_vsync.o(i.hal_internal_video_mode_auto_sync) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_vsync.o(i.hal_internal_video_mode_auto_sync) refers to ceil.o(i.ceil) for ceil
    hal_internal_vsync.o(i.hal_internal_video_mode_auto_sync) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_tear_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_chip_info.o(i.drv_chip_rx_info_check) for drv_chip_rx_info_check
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_rxbr.o(i.drv_rxbr_register_irq0_callback) for drv_rxbr_register_irq0_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_rxbr.o(i.drv_rxbr_register_irq1_callback) for drv_rxbr_register_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_vidc.o(i.drv_vidc_register_callback) for drv_vidc_register_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_init) for dcs_packet_fifo_init
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_gen_te) for soft_gen_te
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_gen_te_double_buffer) for soft_gen_te_double_buffer
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.rxbr_irq0_callback) for rxbr_irq0_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.rxbr_irq1_callback) for rxbr_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.vidc_callback) for vidc_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_register_write_cmd_entry) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) refers to drv_rxbr.o(i.drv_rxbr_set_cmd_filter) for drv_rxbr_set_cmd_filter
    hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) for hal_internal_vsync_set_auto_hw_filter
    hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(i.vsync_set_te_mode) for vsync_set_te_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.vsync_set_te_mode) for vsync_set_te_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg) for drv_rxbr_hline_rcv0_cfg
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to tau_delay.o(i.delayMs) for delayMs
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_vsync.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_set_fs_en_conditions) for drv_memc_set_fs_en_conditions
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_set_lcdc_st_conditions) for drv_memc_set_lcdc_st_conditions
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_set_vidc_sync_cnt) for drv_memc_set_vidc_sync_cnt
    hal_internal_vsync.o(i.hal_internal_vsync_update_lcdc_addr) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dadd.o(.text) for __aeabi_dadd
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area) for hal_dsi_tx_ctrl_set_partial_disp_area
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp) for hal_dsi_tx_ctrl_set_partial_disp
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to drv_param_init.o(i.drv_param_init_get_sclu_filter) for drv_param_init_get_sclu_filter
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to drv_lcdc.o(i.drv_lcdc_config_scale_up_coef) for drv_lcdc_config_scale_up_coef
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_internal_vsync.o(i.hal_internal_init_memc) for hal_internal_init_memc
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(i.dcs_sw_filter) for dcs_sw_filter
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) for dcs_packet_fifo_alloc
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) for hal_dsi_rx_ctrl_dsc_async_handler
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_rxbr.o(i.drv_rxbr_get_col_addr) for drv_rxbr_get_col_addr
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_rxbr.o(i.drv_rxbr_get_page_addr) for drv_rxbr_get_page_addr
    hal_internal_vsync.o(i.rx_partial_update) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_dsc_dec.o(i.drv_dsc_dec_get_nslc) for drv_dsc_dec_get_nslc
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_crgu.o(i.drv_crgu_set_dsco_src) for drv_crgu_set_dsco_src
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_crgu.o(i.drv_crgu_set_dsco_src_div) for drv_crgu_set_dsco_src_div
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_crgu.o(i.drv_crgu_set_dsc_core_div) for drv_crgu_set_dsc_core_div
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rx_partial_update) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(i.rx_get_dcs_packet_data) for rx_get_dcs_packet_data
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(i.rx_receive_pps) for rx_receive_pps
    hal_internal_vsync.o(i.rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_receive_pps) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.rx_receive_pps) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rx_receive_pps) refers to hal_internal_vsync.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter) for drv_dsc_dec_convert_pps_rc_parameter
    hal_internal_vsync.o(i.rx_receive_pps) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps) for drv_dsc_dec_set_u8_pps
    hal_internal_vsync.o(i.rx_receive_pps) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.rx_receive_pps) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.rx_receive_packet) for rx_receive_packet
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_int_source) for drv_rxbr_get_int_source
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.rx_partial_update) for rx_partial_update
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_int_source) for drv_rxbr_get_int_source
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.hal_internal_video_mode_auto_sync) for hal_internal_video_mode_auto_sync
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.vpre_err_reset) for vpre_err_reset
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_memc.o(i.drv_memc_set_double_buffer_reverse) for drv_memc_set_double_buffer_reverse
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.soft_gen_te_double_buffer) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_gen_te_double_buffer) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_get_irq_status) for drv_vidc_get_irq_status
    hal_internal_vsync.o(i.vidc_callback) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_internal_vsync.o(i.vidc_callback) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_clear_irq) for drv_vidc_clear_irq
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_internal_vsync.o(i.vidc_callback) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps) for drv_dsc_dec_set_u8_pps
    hal_internal_vsync.o(i.vpre_err_reset) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to drv_lcdc.o(i.drv_lcdc_ctrl_flow) for drv_lcdc_ctrl_flow
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(.data) refers to hal_internal_vsync.o(.bss) for sg_te_info
    drv_common.o(i.app_HardFault_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_common.o(i.app_SysTick_Handler) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_enable_systick) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_common.o(i.drv_common_enable_systick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_get_tick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_system_init) refers to drv_chip_info.o(i.drv_chip_info_init) for drv_chip_info_init
    drv_common.o(i.drv_common_systick_register_cb) refers to drv_common.o(.data) for .data
    drv_dma.o(i.app_dma_irq_handler) refers to drv_dma.o(i.drv_dma_irq_handler) for drv_dma_irq_handler
    drv_dma.o(i.drv_dma_abort_transfer) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_abort_transfer) refers to drv_dma.o(i.drv_dma_disenable_channel_interrupts) for drv_dma_disenable_channel_interrupts
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_disenable_channel_interrupts) for drv_dma_disenable_channel_interrupts
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_clear_flag) for drv_dma_clear_flag
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_set_ccr) for drv_dma_set_ccr
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_dma.o(i.drv_dma_clear_flag) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.drv_dma_create_handle) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dma.o(i.drv_dma_disenable_channel_interrupts) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.drv_dma_enable_channel_interrupts) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dma.o(i.drv_dma_enable_cycle) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_get_remaining_bytes) refers to drv_dma.o(i.drv_dma_channel_is_active) for drv_dma_channel_is_active
    drv_dma.o(i.drv_dma_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dma.o(i.drv_dma_init) refers to drv_dma.o(i.drv_dma_ahb_init) for drv_dma_ahb_init
    drv_dma.o(i.drv_dma_irq_handler) refers to drv_dma.o(i.drv_dma_get_channel_flag) for drv_dma_get_channel_flag
    drv_dma.o(i.drv_dma_irq_handler) refers to drv_dma.o(i.drv_dma_clear_flag) for drv_dma_clear_flag
    drv_dma.o(i.drv_dma_irq_handler) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_m2m_init) refers to memseta.o(.text) for __aeabi_memclr4
    drv_dma.o(i.drv_dma_m2m_init) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    drv_dma.o(i.drv_dma_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_dma.o(i.drv_dma_set_burst) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_set_transfer) refers to drv_dma.o(i.drv_dma_set_burst) for drv_dma_set_burst
    drv_dma.o(i.drv_dma_start_transfer) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    drv_dma.o(i.drv_dma_start_transfer) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_fls.o(i.drv_fls_gpio_connect) refers to drv_fls.o(i.drv_fls_gpio_disconnect) for drv_fls_gpio_disconnect
    drv_fls.o(i.drv_fls_gpio_disconnect) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_EnableClk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_busy_pending) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    drv_fls.o(i.fls_de_init) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    drv_fls.o(i.fls_de_init) refers to drv_dma.o(i.drv_dma_clear_flag) for drv_dma_clear_flag
    drv_fls.o(i.fls_de_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_disable_it) refers to drv_fls.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_fls.o(i.fls_disable_it) refers to drv_fls.o(i.fls_set_mc_irq_mask) for fls_set_mc_irq_mask
    drv_fls.o(i.fls_enable_it) refers to drv_fls.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_fls.o(i.fls_enable_it) refers to drv_fls.o(i.fls_set_mc_irq_mask) for fls_set_mc_irq_mask
    drv_fls.o(i.fls_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_init) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_spi_init) for fls_spi_init
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_ctrl_cfg_init) for fls_ctrl_cfg_init
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_set_tuning) for fls_set_tuning
    drv_fls.o(i.fls_init) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_enable_it) for fls_enable_it
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_set_mc_irq_mask) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_fls.o(i.fls_set_mc_irq_mask) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_set_write) for fls_set_write
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_set_write) for fls_set_write
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect) for drv_ap_rst_trig_edge_detect
    drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_get_pull_state) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_register_ap_reset_callback) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.drv_gpio_register_callback) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_set_driving_strength) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.drv_gpio_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_gpio.o(i.drv_gpio_set_pull_state) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_set_schmitt_trigger) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_set_slew_rate) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_i2c_dma.o(i.drv_i2c_dma_callback) refers to drv_i2c_dma.o(.data) for .data
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_i2c_master.o(i.drv_i2c_m_enable) for drv_i2c_m_enable
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req) for drv_sys_cfg_set_dma_rx_req
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_dma.o(i.drv_dma_set_transfer) for drv_dma_set_transfer
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_i2c_dma.o(i.drv_i2c_master_write_read_cmd) for drv_i2c_master_write_read_cmd
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_dma.o(i.drv_dma_set_transfer) for drv_dma_set_transfer
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_i2c_dma.o(.data) for .data
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_i2c_dma.o(.bss) for .bss
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_i2c_dma.o(i.drv_i2c_dma_callback) for drv_i2c_dma_callback
    drv_i2c_dma.o(i.drv_i2c_slave_write_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_i2c_master.o(i.app_I2C1_IRQn_Handler) refers to drv_i2c_master.o(.data) for .data
    drv_i2c_master.o(i.drv_i2c1_set_callback) refers to drv_i2c_master.o(.data) for .data
    drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_deinit) refers to drv_i2c_master.o(i.drv_i2c_m_disable_intr) for drv_i2c_m_disable_intr
    drv_i2c_master.o(i.drv_i2c_m_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_i2c_master.o(i.drv_i2c_m_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_i2c_master.o(i.drv_i2c_m_enable_intr) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_read_data) refers to drv_i2c_master.o(i.drv_i2c_m_get_fifo_status) for drv_i2c_m_get_fifo_status
    drv_i2c_master.o(i.drv_i2c_m_set_sys_mask) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_write_data) refers to drv_i2c_master.o(i.drv_i2c_m_get_fifo_status) for drv_i2c_m_get_fifo_status
    drv_i2c_master.o(i.drv_i2c_master_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_i2c_master.o(i.drv_i2c_master_init) refers to drv_common.o(.data) for g_system_clock
    drv_i2c_slave.o(i.app_I2C0_IRQn_Handler) refers to drv_i2c_slave.o(.data) for .data
    drv_i2c_slave.o(i.drv_i2c0_set_callback) refers to drv_i2c_slave.o(.data) for .data
    drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_i2c_slave.o(i.drv_i2c_s_read_data) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    drv_i2c_slave.o(i.drv_i2c_s_set_intr) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_i2c_slave.o(i.drv_i2c_s_set_intr) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_i2c_slave.o(i.drv_i2c_s_write_data) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    drv_i2c_slave.o(i.drv_i2c_slave_init) refers to drv_i2c_slave.o(i.drv_i2c_s_enable) for drv_i2c_s_enable
    drv_param_init.o(i.drv_param_init_get_ccm) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_get_scld_filter_h) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_get_scld_filter_v) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_get_sclu_filter) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_set_ccm) refers to memcpya.o(.text) for __aeabi_memcpy4
    drv_param_init.o(i.drv_param_init_set_ccm) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_set_scld_filter) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_set_sclu_filter) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_p2r_filter_init) refers to drv_param_init.o(.constdata) for .constdata
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_dma.o(i.drv_dma_disenable_channel_interrupts) for drv_dma_disenable_channel_interrupts
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_master.o(i.drv_spi_m_enable_rx_dma) for drv_spi_m_enable_rx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_slave.o(i.drv_spi_s_enable_tx_dma) for drv_spi_s_enable_tx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_slave.o(i.drv_spi_s_enable_rx_dma) for drv_spi_s_enable_rx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_dma.o(i.drv_spi_dma_callback) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_dma_ch6_init) refers to drv_spi_dma.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_dma.o(i.drv_spi_dma_ch6_init) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_dma_init) refers to drv_spi_dma.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_dma.o(i.drv_spi_dma_init) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_spi_dma.o(i.drv_spi_dma_callback) for drv_spi_dma_callback
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_spi_dma.o(i.drv_spi_dma_callback) for drv_spi_dma_callback
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_spi_master.o(i.drv_spi_m_enable_rx_dma) for drv_spi_m_enable_rx_dma
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_spi_slave.o(i.drv_spi_s_enable_tx_dma) for drv_spi_s_enable_tx_dma
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_master.o(i.app_SPIM_IRQn_Handler) refers to drv_spi_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_master.o(i.app_SPIM_IRQn_Handler) refers to drv_spi_master.o(.data) for .data
    drv_spi_master.o(i.drv_spi_m_deinit) refers to drv_spi_master.o(i.drv_spi_m_switch_sclk) for drv_spi_m_switch_sclk
    drv_spi_master.o(i.drv_spi_m_disable_int) refers to drv_spi_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_master.o(i.drv_spi_m_set_intr_callback) refers to drv_spi_master.o(.data) for .data
    drv_spi_master.o(i.drv_spi_master_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_spi_master.o(i.drv_spi_master_init) refers to drv_common.o(.data) for g_system_clock
    drv_swire.o(i.app_SWIRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_swire.o(i.app_SWIRE_IRQn_Handler) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    drv_swire.o(i.app_SWIRE_IRQn_Handler) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_register_callback) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_swire.o(i.drv_swire_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig) for drv_sys_cfg_sel_ap_rst_lvl_trig
    drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect) refers to drv_sys_cfg.o(.data) for .data
    drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig) for drv_sys_cfg_sel_ap_rst_lvl_trig
    drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) refers to drv_sys_cfg.o(.data) for .data
    drv_timer.o(i.app_TIMER0_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.app_TIMER1_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.app_TIMER2_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.app_TIMER3_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_timer.o(i.drv_timer_enable) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_get_instance) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_get_prescaler) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_get_status) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_clear_status_flags) for drv_timer_clear_status_flags
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_register_callback) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_compare_val) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_timer.o(i.drv_timer_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_repeat) refers to drv_timer.o(.data) for .data
    dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_fifo_init) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_size) refers to dcs_packet_fifo.o(.bss) for .bss
    drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to ffltui.o(.text) for __aeabi_ui2f
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fdiv.o(.text) for __aeabi_fdiv
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fmul.o(.text) for __aeabi_fmul
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) for drv_dsi_rx_get_color_bpp
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc) for drv_dsi_rx_get_color_pcc
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fadd.o(.text) for __aeabi_fadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to cfrcmple.o(.text) for __aeabi_cfrcmple
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to f2d.o(.text) for __aeabi_f2d
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dadd.o(.text) for __aeabi_dadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dfixui.o(.text) for __aeabi_d2uiz
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte) for drv_rx_phy_test_write_1_byte
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to drv_dsi_rx.o(i.drv_rx_phy_test_read) for drv_rx_phy_test_read
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap) refers to drv_chip_info.o(i.drv_chip_info_get_info) for drv_chip_info_get_info
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_get_rate_para) for drv_phy_get_rate_para
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_get_calibration) for drv_phy_get_calibration
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_clear) for drv_rx_phy_test_clear
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte) for drv_rx_phy_test_write_1_byte
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte) for drv_rx_phy_test_write_2_byte
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_chip_info.o(i.drv_chip_info_get_info) for drv_chip_info_get_info
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_lock) for drv_rx_phy_test_lock
    drv_dsi_rx.o(i.drv_rx_phy_test_clear) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_rx.o(i.drv_rx_phy_test_lock) refers to drv_phy_common.o(i.drv_phy_test_lock) for drv_phy_test_lock
    drv_dsi_rx.o(i.drv_rx_phy_test_read) refers to drv_phy_common.o(i.drv_phy_test_read) for drv_phy_test_read
    drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_1_byte) for drv_phy_test_write_1_byte
    drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_2_byte) for drv_phy_test_write_2_byte
    drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) for drv_tx_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to drv_dsi_tx.o(i.drv_tx_phy_test_read) for drv_tx_phy_test_read
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_get_rate_para) for drv_phy_get_rate_para
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_get_pll_para) for drv_phy_get_pll_para
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_get_calibration) for drv_phy_get_calibration
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_enter) for drv_tx_phy_test_enter
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_crgu.o(i.drv_crgu_set_mipi_ref_src) for drv_crgu_set_mipi_ref_src
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_crgu.o(i.drv_crgu_set_mipi_cfg_src) for drv_crgu_set_mipi_cfg_src
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_clear) for drv_tx_phy_test_clear
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) for drv_tx_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte) for drv_tx_phy_test_write_2_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_code) for drv_tx_phy_test_write_code
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_exit) for drv_tx_phy_test_exit
    drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) for drv_tx_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_version) for drv_dsi_tx_version
    drv_dsi_tx.o(i.drv_dsi_tx_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_tx.o(i.drv_dsi_tx_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dsi_tx.o(i.drv_tx_phy_test_clear) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_tx.o(i.drv_tx_phy_test_read) refers to drv_phy_common.o(i.drv_phy_test_read) for drv_phy_test_read
    drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_1_byte) for drv_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_2_byte) for drv_phy_test_write_2_byte
    drv_dsi_tx.o(i.drv_tx_phy_test_write_code) refers to drv_phy_common.o(i.drv_phy_test_write_code) for drv_phy_test_write_code
    drv_lcdc.o(i.drv_lcdc_config_src_parameter) refers to drv_lcdc.o(i.drv_lcdc_config_input_size) for drv_lcdc_config_input_size
    drv_lcdc.o(i.drv_lcdc_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_lcdc.o(i.drv_lcdc_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_memc.o(i.app_MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_get_status) for drv_memc_get_status
    drv_memc.o(i.app_MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_clear_status) for drv_memc_clear_status
    drv_memc.o(i.app_MEMC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_rxbr.o(i.app_ADC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.app_ADC_IRQn_Handler) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.app_VPRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.app_VPRE_IRQn_Handler) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_EnableIRQ) for __NVIC_EnableIRQ
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_rxbr.o(i.drv_rxbr_register_irq0_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_register_irq1_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_set_cmd_filter) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_rxbr.o(i.drv_rxbr_soft_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_vidc.o(i.app_VIDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.app_VIDC_IRQn_Handler) refers to drv_vidc.o(.data) for .data
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_vidc.o(i.drv_vidc_register_callback) refers to drv_vidc.o(.data) for .data
    irq_redirect .o(i.ADC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.AP_NRESET_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.DMA_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT0_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT1_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT2_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT3_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT4_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT5_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT6_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT7_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.FLSCTRL_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.HardFault_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.I2C0_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.I2C1_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.LCDC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.MEMC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.MIPI_RX_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.MIPI_TX_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.PWMDET_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SPIM_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SPIS_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SWIRE_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SysTick_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER0_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER1_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER2_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER3_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.UART_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.VIDC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.VPRE_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.WDG_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.handle_init) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.handle_init) refers to drv_common.o(i.app_SysTick_Handler) for app_SysTick_Handler
    irq_redirect .o(i.handle_init) refers to hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) for app_LCDC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler) for app_MIPI_RX_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler) for app_MIPI_TX_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_dma.o(i.app_dma_irq_handler) for app_dma_irq_handler
    irq_redirect .o(i.handle_init) refers to norflash.o(i.app_fls_ctrl_Handler) for app_fls_ctrl_Handler
    irq_redirect .o(i.handle_init) refers to drv_i2c_slave.o(i.app_I2C0_IRQn_Handler) for app_I2C0_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_i2c_master.o(i.app_I2C1_IRQn_Handler) for app_I2C1_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to hal_spi_slave.o(i.app_SPIS_IRQn_Handler) for app_SPIS_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_spi_master.o(i.app_SPIM_IRQn_Handler) for app_SPIM_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_rxbr.o(i.app_VPRE_IRQn_Handler) for app_VPRE_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_rxbr.o(i.app_ADC_IRQn_Handler) for app_ADC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_vidc.o(i.app_VIDC_IRQn_Handler) for app_VIDC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_memc.o(i.app_MEMC_IRQn_Handler) for app_MEMC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER0_IRQn_Handler) for app_TIMER0_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER1_IRQn_Handler) for app_TIMER1_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER2_IRQn_Handler) for app_TIMER2_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER3_IRQn_Handler) for app_TIMER3_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_wdg.o(i.app_WDG_IRQn_Handler) for app_WDG_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_uart.o(i.app_UART_IRQn_Handler) for app_UART_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_pwm.o(i.app_PWMDET_IRQn_Handler) for app_PWMDET_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_swire.o(i.app_SWIRE_IRQn_Handler) for app_SWIRE_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) for app_AP_NRESET_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler) for app_EXTI_INT0_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler) for app_EXTI_INT1_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler) for app_EXTI_INT2_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler) for app_EXTI_INT3_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler) for app_EXTI_INT4_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler) for app_EXTI_INT5_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler) for app_EXTI_INT6_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler) for app_EXTI_INT7_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_common.o(i.app_HardFault_Handler) for app_HardFault_Handler
    drv_efuse.o(i.drv_efuse_enter_inactive) refers to drv_efuse.o(i.drv_efuse_int_enable) for drv_efuse_int_enable
    drv_efuse.o(i.drv_efuse_read) refers to drv_efuse.o(i.drv_efuse_read_req) for drv_efuse_read_req
    drv_efuse.o(i.drv_efuse_write) refers to drv_efuse.o(i.drv_efuse_write_req) for drv_efuse_write_req
    drv_phy_common.o(i.drv_phy_enable_calibration) refers to drv_phy_common.o(.data) for .data
    drv_phy_common.o(i.drv_phy_get_calibration) refers to drv_chip_info.o(i.drv_chip_info_get_info) for drv_chip_info_get_info
    drv_phy_common.o(i.drv_phy_get_calibration) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_phy_common.o(i.drv_phy_get_calibration) refers to drv_phy_common.o(.data) for .data
    drv_phy_common.o(i.drv_phy_get_pll_para) refers to drv_phy_common.o(.constdata) for .constdata
    drv_phy_common.o(i.drv_phy_get_rate_para) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_phy_common.o(i.drv_phy_get_rate_para) refers to drv_phy_common.o(.constdata) for .constdata
    drv_phy_common.o(i.drv_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_code) for drv_phy_test_write_code
    drv_phy_common.o(i.drv_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_data) for drv_phy_test_write_data
    drv_phy_common.o(i.drv_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_code) for drv_phy_test_write_code
    drv_phy_common.o(i.drv_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_data) for drv_phy_test_write_data
    drv_chip_info.o(i.drv_chip_info_get_info) refers to drv_chip_info.o(.data) for .data
    drv_chip_info.o(i.drv_chip_info_init) refers to drv_efuse.o(i.drv_efuse_enter_inactive) for drv_efuse_enter_inactive
    drv_chip_info.o(i.drv_chip_info_init) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_chip_info.o(i.drv_chip_info_init) refers to drv_chip_info.o(.data) for .data
    drv_chip_info.o(i.drv_chip_rx_info_check) refers to printfa.o(i.__0printf) for __2printf
    drv_chip_info.o(i.drv_chip_rx_info_check) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_chip_info.o(i.drv_chip_rx_info_check) refers to drv_chip_info.o(.data) for .data
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to drv_efuse.o(i.drv_efuse_enter_inactive) for drv_efuse_enter_inactive
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to printfa.o(i.__0printf) for __2printf
    tau_log.o(i.LOG_printf) refers to printfa.o(i.__0vsprintf) for vsprintf
    tau_log.o(i.LOG_printf) refers to printfa.o(i.__0printf) for __2printf
    tau_log.o(i.LOG_printf) refers to tau_log.o(.bss) for .bss
    tau_log.o(i.fgetc) refers to hal_uart.o(i.hal_uart_receive_blocking) for hal_uart_receive_blocking
    tau_log.o(i.fputc) refers to hal_uart.o(i.hal_uart_transmit_blocking) for hal_uart_transmit_blocking
    app_tp_enc.o(i.EncryptCheck) refers to app_tp_enc.o(.data) for .data
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to ap_demo.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to hal_spi_slave.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_spi_slave.o(i.hal_spi_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    hal_spi_slave.o(i.hal_spi_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_abort) refers to drv_spi_dma.o(i.drv_spi_abort_dma) for drv_spi_abort_dma
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start) refers to drv_dma.o(i.drv_dma_enable_cycle) for drv_dma_enable_cycle
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start) refers to drv_spi_dma.o(i.drv_spis_dma_write) for drv_spis_dma_write
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_deinit) refers to drv_spi_slave.o(i.drv_spi_s_deinit) for drv_spi_s_deinit
    hal_spi_slave.o(i.hal_spi_slave_enable) refers to drv_spi_slave.o(i.drv_spi_s_enable_int) for drv_spi_s_enable_int
    hal_spi_slave.o(i.hal_spi_slave_enable) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_spi_slave.o(i.hal_spi_slave_enable) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_gpio_init) refers to drv_spi_slave.o(i.drv_spi_s_gpio_init) for drv_spi_s_gpio_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to hal_spi_slave.o(i.hal_spi_slave_gpio_init) for hal_spi_slave_gpio_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_slave.o(i.drv_spi_slave_init) for drv_spi_slave_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_dma.o(i.drv_spi_dma_init) for drv_spi_dma_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) for drv_spi_set_dma_irq_callback
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_slave.o(i.drv_spi_s_enable_tx_dma) for drv_spi_s_enable_tx_dma
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    hal_spi_slave.o(i.hal_spi_slave_init) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_read_data) refers to drv_spi_slave.o(i.drv_spi_s_read_data) for drv_spi_s_read_data
    hal_spi_slave.o(i.hal_spi_slave_register_callback) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_reset_tx) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_set_auto_rx_buffer) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_set_auto_tx_buffer) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_write_data) refers to drv_spi_slave.o(i.drv_spi_s_write_data) for drv_spi_s_write_data
    norflash.o(i.app_fls_ctrl_Handler) refers to drv_fls.o(i.fls_clr_interrupt_flag) for fls_clr_interrupt_flag
    norflash.o(i.app_fls_ctrl_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    norflash.o(i.app_fls_ctrl_Handler) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_best_cfg_init) refers to drv_fls.o(i.fls_spi_init) for fls_spi_init
    norflash.o(i.norflash_best_cfg_init) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_check_id) refers to norflash.o(i.norflash_read_id) for norflash_read_id
    norflash.o(i.norflash_check_id) refers to tau_delay.o(i.delayUs) for delayUs
    norflash.o(i.norflash_check_id) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dma_callback) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dma_read) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_transfer_create_handle_dma) for fls_transfer_create_handle_dma
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_dma_read_prepare) for fls_dma_read_prepare
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_transfer_dma) for fls_transfer_dma
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    norflash.o(i.norflash_dma_read) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dma_read) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_dma_read) refers to norflash.o(i.norflash_dma_callback) for norflash_dma_callback
    norflash.o(i.norflash_dma_write) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_transfer_create_handle_dma) for fls_transfer_create_handle_dma
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_switch_fls_spi) for norflash_switch_fls_spi
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_dma_write_prepare) for fls_dma_write_prepare
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_transfer_dma) for fls_transfer_dma
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    norflash.o(i.norflash_dma_write) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_dma_write) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_dma_callback) for norflash_dma_callback
    norflash.o(i.norflash_dma_write) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dual_read) refers to drv_fls.o(i.fls_ddat_enable) for fls_ddat_enable
    norflash.o(i.norflash_dual_read) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_dual_read) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_switch_fls_spi) for norflash_switch_fls_spi
    norflash.o(i.norflash_dual_write) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_dual_write) refers to drv_fls.o(i.fls_ddat_enable) for fls_ddat_enable
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_en4b) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_read_config_reg) for norflash_read_config_reg
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_en_quad) refers to norflash.o(i.norflash_en_quad_check) for norflash_en_quad_check
    norflash.o(i.norflash_en_quad) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_en_quad) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_en_quad) refers to drv_fls.o(i.fls_busy_pending) for fls_busy_pending
    norflash.o(i.norflash_en_quad) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(i.norflash_get_dual_hstatus) for norflash_get_dual_hstatus
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(i.norflash_get_hstatus) for norflash_get_hstatus
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_erase_block) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_erase_block) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_erase_block) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_erase_block) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_erase_chip) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_erase_chip) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_erase_chip) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_erase_sector) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_erase_sector) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_erase_sector) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_erase_sector) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_ex4b) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_read_config_reg) for norflash_read_config_reg
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_exit_quad) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_exit_quad) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_exit_quad) refers to norflash.o(i.norflash_en_quad_check) for norflash_en_quad_check
    norflash.o(i.norflash_exit_quad) refers to drv_fls.o(i.fls_busy_pending) for fls_busy_pending
    norflash.o(i.norflash_exit_quad) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_get_dual_hstatus) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_get_dual_hstatus) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_get_dual_hstatus) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_get_hstatus) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_get_hstatus) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_get_hstatus) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_get_status) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_get_status) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_get_status) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_get_default_spi_config) for fls_get_default_spi_config
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_get_default_fls_config) for fls_get_default_fls_config
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_get_default_tuning) for fls_get_default_tuning
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_init) for fls_init
    norflash.o(i.norflash_init) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_init) refers to drv_fls.o(.data) for g_fls_tuning
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_qdat_enable) for fls_qdat_enable
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_qadr_enable) for fls_qadr_enable
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_qcmd_enable) for fls_qcmd_enable
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_switch_fls_spi) for norflash_switch_fls_spi
    norflash.o(i.norflash_quad_write) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_quad_write) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_read) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_read_config_reg) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_read_id) refers to drv_fls.o(i.fls_read_cmd) for fls_read_cmd
    norflash.o(i.norflash_read_uid) refers to memseta.o(.text) for __aeabi_memclr4
    norflash.o(i.norflash_read_uid) refers to drv_fls.o(i.fls_read_cmd) for fls_read_cmd
    norflash.o(i.norflash_read_uid) refers to memcpya.o(.text) for __aeabi_memcpy
    norflash.o(i.norflash_set_best_cfg) refers to memseta.o(.text) for __aeabi_memclr4
    norflash.o(i.norflash_set_best_read_cfg) refers to norflash.o(i.norflash_en_quad) for norflash_en_quad
    norflash.o(i.norflash_set_best_read_cfg) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_set_best_read_cfg) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_set_best_write_cfg) refers to norflash.o(i.norflash_en_quad) for norflash_en_quad
    norflash.o(i.norflash_set_best_write_cfg) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_set_best_write_cfg) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_ddat_enable) for fls_ddat_enable
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_qdat_enable) for fls_qdat_enable
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_qadr_enable) for fls_qadr_enable
    norflash.o(i.norflash_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_write) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_write_disable) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_write_disable) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write_disable) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_write_disable) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_write_enable) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_write_enable) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write_enable) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_write_enable) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_big_end_enable) for norflash_big_end_enable
    norflash.o(i.norflash_write_endian_scr) refers to drv_fls.o(i.fls_en_scr) for fls_en_scr
    norflash.o(i.norflash_write_endian_scr) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_big_end_clear) for norflash_big_end_clear
    norflash.o(i.norflash_write_endian_scr) refers to drv_fls.o(i.fls_scr_clear) for fls_scr_clear
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    drv_fls_dma.o(i.fls_abort_dma) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_fls_dma.o(i.fls_abort_dma) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls_dma.o(i.fls_dma_enable) for fls_dma_enable
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_set_write) for fls_set_write
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls_dma.o(i.fls_dma_enable) for fls_dma_enable
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls_dma.o(i.fls_read_dmacallback) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to memseta.o(.text) for __aeabi_memclr4
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_fls_dma.o(.data) for .data
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_fls_dma.o(i.fls_read_dmacallback) for fls_read_dmacallback
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_fls_dma.o(i.fls_write_dmacallback) for fls_write_dmacallback
    drv_fls_dma.o(i.fls_transfer_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_fls_dma.o(i.fls_transfer_dma) refers to drv_dma.o(i.drv_dma_start_transfer) for drv_dma_start_transfer
    drv_fls_dma.o(i.fls_transfer_get_receive_count_dma) refers to drv_dma.o(i.drv_dma_get_remaining_bytes) for drv_dma_get_remaining_bytes
    drv_fls_dma.o(i.fls_write_dmacallback) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_pwm.o(i.app_PWMDET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_pwm.o(i.app_PWMDET_IRQn_Handler) refers to drv_pwm.o(.data) for .data
    drv_pwm.o(i.drv_pwm_in_register_callback) refers to drv_pwm.o(.data) for .data
    drv_pwm.o(i.drv_pwm_in_set_sys_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_pwm.o(i.drv_pwm_in_set_sys_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_spi_slave.o(i.drv_spi_s_deinit) refers to drv_spi_slave.o(i.drv_spi_s_switch_sclk) for drv_spi_s_switch_sclk
    drv_uart.o(i.UART0_IRQ_Handle) refers to drv_uart.o(i.UART_TransferHandleIRQ) for UART_TransferHandleIRQ
    drv_uart.o(i.UART0_IRQ_Handle) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_uart.o(i.UART0_IRQ_Handle) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_AbortReceive) refers to drv_uart.o(i.UART_Disable_IT) for UART_Disable_IT
    drv_uart.o(i.UART_AbortReceive) refers to drv_uart.o(i.UART_ResetRxFIFO) for UART_ResetRxFIFO
    drv_uart.o(i.UART_AbortSend) refers to drv_uart.o(i.UART_Disable_IT) for UART_Disable_IT
    drv_uart.o(i.UART_AbortSend) refers to drv_uart.o(i.UART_ResetTxFIFO) for UART_ResetTxFIFO
    drv_uart.o(i.UART_Deinit) refers to drv_uart.o(i.UART_SwitchSCLK) for UART_SwitchSCLK
    drv_uart.o(i.UART_Disable_IT) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_Disable_IT) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.UART_Disable_IT) refers to drv_uart.o(.constdata) for .constdata
    drv_uart.o(i.UART_EnableDma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req) for drv_sys_cfg_set_dma_rx_req
    drv_uart.o(i.UART_EnableDma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    drv_uart.o(i.UART_Enable_IT) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_Enable_IT) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.UART_GetDefaultConfig) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.UART_GetDefaultConfig) refers to drv_common.o(.data) for g_system_clock
    drv_uart.o(i.UART_GetFIFO_Ctrl) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_GetFIFO_Ctrl) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_ResetRxFIFO) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_ResetRxFIFO) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_ResetTxFIFO) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_ResetTxFIFO) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_SetBaudRate) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_uart.o(i.UART_SwitchSCLK) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_uart.o(i.UART_TransferCreateHandle) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_TransferCreateHandle) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.UART_TransferCreateHandle) refers to drv_uart.o(i.UART_Enable_IT) for UART_Enable_IT
    drv_uart.o(i.UART_TransferCreateHandle) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_TransferHandleIRQ) refers to drv_uart.o(i.UART_ResetRxFIFO) for UART_ResetRxFIFO
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_DisableDma) for UART_DisableDma
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_SwitchSCLK) for UART_SwitchSCLK
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_SetBaudRate) for UART_SetBaudRate
    drv_uart.o(i.UART_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.UART_init) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.app_UART_IRQn_Handler) refers to drv_uart.o(i.UART0_IRQ_Handle) for UART0_IRQ_Handle
    drv_uart_dma.o(i.UART_DMAInit) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart_dma.o(i.UART_DMAInit) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    drv_uart_dma.o(i.UART_TransferAbortReceiveDMA) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_uart_dma.o(i.UART_TransferAbortSendDMA) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart.o(i.UART_EnableDma) for UART_EnableDma
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(i.UART_DMAInit) for UART_DMAInit
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(.data) for .data
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(i.UART_TransferReceiveDMACallback) for UART_TransferReceiveDMACallback
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(i.UART_TransferSendDMACallback) for UART_TransferSendDMACallback
    drv_uart_dma.o(i.UART_TransferGetReceiveCountDMA) refers to drv_dma.o(i.drv_dma_get_remaining_bytes) for drv_dma_get_remaining_bytes
    drv_uart_dma.o(i.UART_TransferReceiveDMA) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_uart_dma.o(i.UART_TransferReceiveDMA) refers to drv_uart.o(i.UART_EnableDma) for UART_EnableDma
    drv_uart_dma.o(i.UART_TransferReceiveDMA) refers to drv_dma.o(i.drv_dma_start_transfer) for drv_dma_start_transfer
    drv_uart_dma.o(i.UART_TransferSendDMA) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_uart_dma.o(i.UART_TransferSendDMA) refers to drv_uart.o(i.UART_EnableDma) for UART_EnableDma
    drv_uart_dma.o(i.UART_TransferSendDMA) refers to drv_dma.o(i.drv_dma_start_transfer) for drv_dma_start_transfer
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_set_int) for drv_wdg_set_int
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_clear_counter) for drv_wdg_clear_counter
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_read_edge_flag) for drv_wdg_read_edge_flag
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_clear_edge_flag) for drv_wdg_clear_edge_flag
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(.data) for .data
    drv_wdg.o(i.drv_wdg_register_callback) refers to drv_wdg.o(.data) for .data
    drv_wdg.o(i.drv_wdg_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_wdg.o(i.drv_wdg_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_wdg.o(i.drv_wdg_set_repeat) refers to drv_wdg.o(.data) for .data
    ceil.o(i.__softfp_ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.__softfp_ceil) refers to ceil.o(i.ceil) for ceil
    ceil.o(i.ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.ceil) refers to dadd.o(.text) for __aeabi_dadd
    ceil.o(i.ceil) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    sqrt.o(i.__softfp_sqrt) refers (Special) to iusefp.o(.text) for __I$use$fp
    sqrt.o(i.__softfp_sqrt) refers to dsqrt.o(.text) for _dsqrt
    sqrt.o(i.__softfp_sqrt) refers to errno.o(i.__set_errno) for __set_errno
    sqrt.o(i.sqrt) refers (Special) to iusefp.o(.text) for __I$use$fp
    sqrt.o(i.sqrt) refers to dsqrt.o(.text) for _dsqrt
    sqrt.o(i.sqrt) refers to errno.o(i.__set_errno) for __set_errno
    sqrt_x.o(i.____softfp_sqrt$lsc) refers (Special) to iusefp.o(.text) for __I$use$fp
    sqrt_x.o(i.____softfp_sqrt$lsc) refers to cdcmple.o(.text) for __aeabi_cdcmple
    sqrt_x.o(i.____softfp_sqrt$lsc) refers to errno.o(i.__set_errno) for __set_errno
    sqrt_x.o(i.____softfp_sqrt$lsc) refers to dsqrt.o(.text) for _dsqrt
    sqrt_x.o(i.__sqrt$lsc) refers (Special) to iusefp.o(.text) for __I$use$fp
    sqrt_x.o(i.__sqrt$lsc) refers to cdcmple.o(.text) for __aeabi_cdcmple
    sqrt_x.o(i.__sqrt$lsc) refers to errno.o(i.__set_errno) for __set_errno
    sqrt_x.o(i.__sqrt$lsc) refers to dsqrt.o(.text) for _dsqrt
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry10a.o(.ARM.Collect$$$$0000000D) for __rt_final_cpp
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry11a.o(.ARM.Collect$$$$0000000F) for __rt_final_exit
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry7b.o(.ARM.Collect$$$$00000008) for _main_clock
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry8b.o(.ARM.Collect$$$$0000000A) for _main_cpp_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry9a.o(.ARM.Collect$$$$0000000B) for _main_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry5.o(.ARM.Collect$$$$00000004) for _main_scatterload
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry2.o(.ARM.Collect$$$$00000001) for _main_stk
    idiv.o(.text) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfb.o(i.__0fprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0fprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0printf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printfb.o(i.__0vfprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vfprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printf0.o(i.__0fprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0fprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0printf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf0.o(i.__0vfprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vfprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf1.o(i.__0fprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0fprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0printf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i.__0vfprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vfprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf2.o(i.__0fprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0fprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0printf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf2.o(i.__0vfprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vfprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf3.o(i.__0fprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0fprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0printf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i.__0vfprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vfprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf4.o(i.__0fprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0fprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0printf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i.__0vfprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vfprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf5.o(i.__0fprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0fprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0printf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i.__0vfprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vfprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf6.o(i.__0fprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0fprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0printf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i.__0vfprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vfprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i._printf_core) refers to printf6.o(i._printf_pre_padding) for _printf_pre_padding
    printf6.o(i._printf_core) refers to printf6.o(i._printf_post_padding) for _printf_post_padding
    printf6.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf7.o(i.__0fprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0fprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0printf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i.__0vfprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vfprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i._printf_core) refers to printf7.o(i._printf_pre_padding) for _printf_pre_padding
    printf7.o(i._printf_core) refers to printf7.o(i._printf_post_padding) for _printf_post_padding
    printf7.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf8.o(i.__0fprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0fprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0printf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i.__0vfprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vfprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i._printf_core) refers to printf8.o(i._printf_pre_padding) for _printf_pre_padding
    printf8.o(i._printf_core) refers to printf8.o(i._printf_post_padding) for _printf_post_padding
    printf8.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i.__0fprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0fprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0fprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0printf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0printf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0snprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0snprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0snprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0sprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0sprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0sprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i.__0vfprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vfprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vfprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0vsnprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0vsprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i._fp_digits) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._fp_digits) refers to dmul.o(.text) for __aeabi_dmul
    printfa.o(i._fp_digits) refers to ddiv.o(.text) for __aeabi_ddiv
    printfa.o(i._fp_digits) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    printfa.o(i._fp_digits) refers to dadd.o(.text) for __aeabi_dadd
    printfa.o(i._fp_digits) refers to dfixul.o(.text) for __aeabi_d2ulz
    printfa.o(i._fp_digits) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_core) refers to printfa.o(i._printf_pre_padding) for _printf_pre_padding
    printfa.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers to printfa.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i._printf_core) refers to printfa.o(i._fp_digits) for _fp_digits
    printfa.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfa.o(i._printf_post_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_pre_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._snputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._sputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    fmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers to fepilogue.o(.text) for _float_round
    fscalb.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    dadd.o(.text) refers to llsshr.o(.text) for __aeabi_lasr
    dadd.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dmul.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ddiv.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ddiv.o(.text) refers to depilogue.o(.text) for _double_round
    fflti.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fflti.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    ffltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ffltui.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    dflti.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dflti.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dfltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfltui.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ffixi.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ffixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixi.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixi.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixui.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    f2d.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    cdcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    cfrcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    entry2.o(.ARM.Collect$$$$00000001) refers to entry2.o(.ARM.Collect$$$$00002712) for __lit__00000000
    entry2.o(.ARM.Collect$$$$00002712) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    entry5.o(.ARM.Collect$$$$00000004) refers to init.o(.text) for __scatterload
    entry9a.o(.ARM.Collect$$$$0000000B) refers to main.o(i.main) for main
    entry9b.o(.ARM.Collect$$$$0000000C) refers to main.o(i.main) for main
    uldiv.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    uldiv.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    errno.o(i.__aeabi_errno_addr) refers to errno.o(.data) for .data
    errno.o(i.__read_errno) refers to errno.o(.data) for .data
    errno.o(i.__set_errno) refers to errno.o(.data) for .data
    depilogue.o(.text) refers to depilogue.o(i.__ARM_clz) for __ARM_clz
    depilogue.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dsqrt.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dsqrt.o(.text) refers to depilogue.o(.text) for _double_round
    dfixul.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixul.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    init.o(.text) refers to entry5.o(.ARM.Collect$$$$00000004) for __main_after_scatterload


==============================================================================

Removing Unused input sections from the image.

    Removing main.o(.rev16_text), (4 bytes).
    Removing main.o(.revsh_text), (4 bytes).
    Removing ap_demo.o(.rev16_text), (4 bytes).
    Removing ap_demo.o(.revsh_text), (4 bytes).
    Removing ap_demo.o(.data), (1 bytes).
    Removing ap_demo.o(.data), (4 bytes).
    Removing app_tp_transfer.o(.rev16_text), (4 bytes).
    Removing app_tp_transfer.o(.revsh_text), (4 bytes).
    Removing app_tp_transfer.o(i.app_tp_m_transfer_complate), (8 bytes).
    Removing app_tp_transfer.o(i.app_tp_phone_reset_on), (12 bytes).
    Removing app_tp_transfer.o(i.app_tp_s_transfer_complate), (26 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (5 bytes).
    Removing app_tp_transfer.o(.data), (6 bytes).
    Removing app_tp_transfer.o(.data), (2 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (1 bytes).
    Removing app_tp_transfer.o(.data), (2 bytes).
    Removing app_tp_transfer.o(.data), (2 bytes).
    Removing app_tp_st_touch.o(.rev16_text), (4 bytes).
    Removing app_tp_st_touch.o(.revsh_text), (4 bytes).
    Removing app_tp_st_touch.o(i.CRC16_2), (64 bytes).
    Removing app_tp_st_touch.o(i.ap_set_tp_calibration_04), (152 bytes).
    Removing app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset), (136 bytes).
    Removing app_tp_st_touch.o(.constdata), (32 bytes).
    Removing board.o(.rev16_text), (4 bytes).
    Removing board.o(.revsh_text), (4 bytes).
    Removing startup_armcm0.o(HEAP), (3072 bytes).
    Removing hal_dsi_rx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd), (88 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_short_cmd), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video), (228 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init), (48 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern), (216 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en), (16 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle), (40 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart), (80 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk), (44 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter), (108 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_dcs_direct_mode), (8 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter), (40 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format), (56 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data), (148 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data), (268 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk), (68 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_te_waveform), (52 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate), (10 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution_ex), (32 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_register_write_cmd_entry), (110 bytes).
    Removing hal_dsi_tx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic), (148 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode_rcv_te), (10 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard), (280 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker), (172 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_mode_init), (30 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_ulps_mode), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_ulps_mode), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd), (140 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle), (28 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_pq_filter), (28 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_lp_cmd), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data), (272 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg), (80 bytes).
    Removing hal_gpio.o(.rev16_text), (4 bytes).
    Removing hal_gpio.o(.revsh_text), (4 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_int_type), (20 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_pull_state), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_driving_strength), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_output_data_ex), (36 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_schmitt_trigger), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_slew_rate), (32 bytes).
    Removing hal_i2c_master.o(.rev16_text), (4 bytes).
    Removing hal_i2c_master.o(.revsh_text), (4 bytes).
    Removing hal_i2c_master.o(i.hal_i2c_m_deinit), (8 bytes).
    Removing hal_i2c_master.o(i.hal_i2c_m_set_high_impedance), (46 bytes).
    Removing hal_i2c_slave.o(.rev16_text), (4 bytes).
    Removing hal_i2c_slave.o(.revsh_text), (4 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_deinit), (88 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_get_tx_byte_num), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_read_complate), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_read_complate_clear), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_read_data), (32 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_rxfifo_notempty), (40 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_sel), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_set_dma_tx_cycle), (36 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance), (88 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_write_complate), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_write_data), (32 bytes).
    Removing hal_spi_master.o(.rev16_text), (4 bytes).
    Removing hal_spi_master.o(.revsh_text), (4 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_callback), (24 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_deinit), (10 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_dma_init), (104 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_dma_read), (36 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_dma_write), (40 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_get_transfer_complate), (36 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_gpio_init), (8 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_read_rxfifo), (28 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_set_high_impedance), (100 bytes).
    Removing hal_spi_master.o(.data), (1 bytes).
    Removing hal_swire.o(.rev16_text), (4 bytes).
    Removing hal_swire.o(.revsh_text), (4 bytes).
    Removing hal_swire.o(i.hal_swire_deinit), (18 bytes).
    Removing hal_swire.o(i.hal_swire_init), (32 bytes).
    Removing hal_swire.o(i.hal_swire_register_callback), (10 bytes).
    Removing hal_swire.o(i.hal_swire_start), (108 bytes).
    Removing hal_system.o(.rev16_text), (4 bytes).
    Removing hal_system.o(.revsh_text), (4 bytes).
    Removing hal_system.o(i.hal_system_clear_debug_state), (10 bytes).
    Removing hal_system.o(i.hal_system_deep_sleep_mode), (8 bytes).
    Removing hal_system.o(i.hal_system_disable_systick), (8 bytes).
    Removing hal_system.o(i.hal_system_get_debug_state), (8 bytes).
    Removing hal_system.o(i.hal_system_get_tick), (8 bytes).
    Removing hal_system.o(i.hal_system_idle_mode), (8 bytes).
    Removing hal_system.o(i.hal_system_register_systick_cb), (8 bytes).
    Removing hal_system.o(i.hal_system_reset_chip), (32 bytes).
    Removing hal_system.o(i.hal_system_share_flash_mode), (20 bytes).
    Removing hal_system.o(i.hal_system_sleep_mode), (48 bytes).
    Removing hal_timer.o(.rev16_text), (4 bytes).
    Removing hal_timer.o(.revsh_text), (4 bytes).
    Removing hal_timer.o(i.hal_timer_deinit), (46 bytes).
    Removing hal_timer.o(i.hal_timer_get_status), (8 bytes).
    Removing hal_timer.o(i.hal_timer_set_repeat), (8 bytes).
    Removing hal_timer.o(i.hal_timer_start_ex), (72 bytes).
    Removing tau_delay.o(.rev16_text), (4 bytes).
    Removing tau_delay.o(.revsh_text), (4 bytes).
    Removing app_tp_for_custom_s8.o(.rev16_text), (4 bytes).
    Removing app_tp_for_custom_s8.o(.revsh_text), (4 bytes).
    Removing app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const), (56 bytes).
    Removing app_tp_for_custom_s8.o(.bss), (200 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (37 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (1 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (3 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (3 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (11 bytes).
    Removing app_tp_for_custom_s8.o(.data), (10 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (64 bytes).
    Removing app_tp_for_custom_s8.o(.data), (3 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (32 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing hal_uart.o(.rev16_text), (4 bytes).
    Removing hal_uart.o(.revsh_text), (4 bytes).
    Removing hal_uart.o(i.hal_uart_deinit), (28 bytes).
    Removing hal_uart.o(i.hal_uart_dmacallback), (36 bytes).
    Removing hal_uart.o(i.hal_uart_receive_blocking), (16 bytes).
    Removing hal_uart.o(i.hal_uart_receive_dma), (76 bytes).
    Removing hal_uart.o(i.hal_uart_transmit_dma), (76 bytes).
    Removing hal_internal_vsync.o(.rev16_text), (4 bytes).
    Removing hal_internal_vsync.o(.revsh_text), (4 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te), (168 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex), (468 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual), (528 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_register_write_cmd_entry), (12 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode), (48 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate), (680 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_update_lcdc_addr), (48 bytes).
    Removing hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler), (476 bytes).
    Removing drv_common.o(.rev16_text), (4 bytes).
    Removing drv_common.o(.revsh_text), (4 bytes).
    Removing drv_common.o(i.drv_common_disable_systick), (20 bytes).
    Removing drv_common.o(i.drv_common_get_tick), (12 bytes).
    Removing drv_common.o(i.drv_common_idle_mode), (40 bytes).
    Removing drv_common.o(i.drv_common_systick_register_cb), (12 bytes).
    Removing drv_crgu.o(.rev16_text), (4 bytes).
    Removing drv_crgu.o(.revsh_text), (4 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_all_reset_flags), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_reset_flag), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_config_clocks), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_config_clocks_div), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_config_clocks_src), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_ana_clk_status), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_clocks), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_fpga_id), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_mipi_ref_src), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_reset_flag), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_system_clk), (28 bytes).
    Removing drv_crgu.o(i.drv_crgu_reset_chip), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_200m_scan_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_300m_scan_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_abp0_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_adc_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_adc_src), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_apb1_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_apb2_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_fls_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_fls_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_monitor_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_monitor_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_swire_div), (20 bytes).
    Removing drv_dma.o(.rev16_text), (4 bytes).
    Removing drv_dma.o(.revsh_text), (4 bytes).
    Removing drv_dma.o(i.drv_dma_abort_transfer), (32 bytes).
    Removing drv_dma.o(i.drv_dma_ahb_init), (74 bytes).
    Removing drv_dma.o(i.drv_dma_channel_is_active), (20 bytes).
    Removing drv_dma.o(i.drv_dma_deinit), (32 bytes).
    Removing drv_dma.o(i.drv_dma_disenable_channel_interrupts), (24 bytes).
    Removing drv_dma.o(i.drv_dma_enable_cycle), (44 bytes).
    Removing drv_dma.o(i.drv_dma_get_remaining_bytes), (32 bytes).
    Removing drv_dma.o(i.drv_dma_init), (24 bytes).
    Removing drv_dma.o(i.drv_dma_m2m_init), (72 bytes).
    Removing drv_dma.o(i.drv_dma_reset), (10 bytes).
    Removing drv_dma.o(i.drv_dma_set_ccr), (114 bytes).
    Removing drv_dma.o(i.drv_dma_start_transfer), (32 bytes).
    Removing drv_fls.o(.rev16_text), (4 bytes).
    Removing drv_fls.o(.revsh_text), (4 bytes).
    Removing drv_fls.o(i.__NVIC_DisableIRQ), (32 bytes).
    Removing drv_fls.o(i.drv_fls_gpio_connect), (28 bytes).
    Removing drv_fls.o(i.drv_fls_gpio_disconnect), (32 bytes).
    Removing drv_fls.o(i.fls_EnableClk), (12 bytes).
    Removing drv_fls.o(i.fls_busy_pending), (12 bytes).
    Removing drv_fls.o(i.fls_clear_irq_status), (6 bytes).
    Removing drv_fls.o(i.fls_ctrl_cfg_init), (72 bytes).
    Removing drv_fls.o(i.fls_ddat_enable), (24 bytes).
    Removing drv_fls.o(i.fls_de_init), (52 bytes).
    Removing drv_fls.o(i.fls_descr), (10 bytes).
    Removing drv_fls.o(i.fls_disable_it), (36 bytes).
    Removing drv_fls.o(i.fls_en_scr), (10 bytes).
    Removing drv_fls.o(i.fls_enable_it), (48 bytes).
    Removing drv_fls.o(i.fls_get_crcout), (4 bytes).
    Removing drv_fls.o(i.fls_get_default_fls_config), (20 bytes).
    Removing drv_fls.o(i.fls_get_default_spi_config), (44 bytes).
    Removing drv_fls.o(i.fls_get_default_tuning), (12 bytes).
    Removing drv_fls.o(i.fls_get_tuning), (18 bytes).
    Removing drv_fls.o(i.fls_init), (62 bytes).
    Removing drv_fls.o(i.fls_qadr_enable), (22 bytes).
    Removing drv_fls.o(i.fls_qcmd_enable), (22 bytes).
    Removing drv_fls.o(i.fls_qdat_enable), (22 bytes).
    Removing drv_fls.o(i.fls_read_byte_data), (130 bytes).
    Removing drv_fls.o(i.fls_read_cmd), (104 bytes).
    Removing drv_fls.o(i.fls_read_cmd_it), (110 bytes).
    Removing drv_fls.o(i.fls_reset_crc), (18 bytes).
    Removing drv_fls.o(i.fls_scr_clear), (10 bytes).
    Removing drv_fls.o(i.fls_set_addr_dummy), (32 bytes).
    Removing drv_fls.o(i.fls_set_addr_len), (32 bytes).
    Removing drv_fls.o(i.fls_set_mc_irq_mask), (26 bytes).
    Removing drv_fls.o(i.fls_set_read), (10 bytes).
    Removing drv_fls.o(i.fls_set_tuning), (24 bytes).
    Removing drv_fls.o(i.fls_set_write), (10 bytes).
    Removing drv_fls.o(i.fls_single_mode), (16 bytes).
    Removing drv_fls.o(i.fls_spi_init), (180 bytes).
    Removing drv_fls.o(i.fls_spi_start), (10 bytes).
    Removing drv_fls.o(i.fls_swrst), (18 bytes).
    Removing drv_fls.o(i.fls_write_byte_data), (164 bytes).
    Removing drv_fls.o(i.fls_write_cmd), (58 bytes).
    Removing drv_fls.o(.data), (4 bytes).
    Removing drv_gpio.o(.rev16_text), (4 bytes).
    Removing drv_gpio.o(.revsh_text), (4 bytes).
    Removing drv_gpio.o(i.drv_gpio_get_pull_state), (224 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_driving_strength), (312 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_schmitt_trigger), (168 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_slew_rate), (168 bytes).
    Removing drv_i2c_dma.o(.rev16_text), (4 bytes).
    Removing drv_i2c_dma.o(.revsh_text), (4 bytes).
    Removing drv_i2c_master.o(.rev16_text), (4 bytes).
    Removing drv_i2c_master.o(.revsh_text), (4 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_bus_init), (36 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_deinit), (44 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_disable_intr), (16 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_get_fifo_status), (28 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_read_data), (32 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_set_fifo_threshold), (24 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_set_sys_mask), (48 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_write_data), (32 bytes).
    Removing drv_i2c_slave.o(.rev16_text), (4 bytes).
    Removing drv_i2c_slave.o(.revsh_text), (4 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_read_data), (30 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_set_fifo_threshold), (16 bytes).
    Removing drv_param_init.o(.rev16_text), (4 bytes).
    Removing drv_param_init.o(.revsh_text), (4 bytes).
    Removing drv_param_init.o(i.drv_param_init_set_scld_filter), (100 bytes).
    Removing drv_param_init.o(i.drv_param_init_set_sclu_filter), (28 bytes).
    Removing drv_pwr.o(.rev16_text), (4 bytes).
    Removing drv_pwr.o(.revsh_text), (4 bytes).
    Removing drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_frame_buff_pd), (28 bytes).
    Removing drv_spi_dma.o(.rev16_text), (4 bytes).
    Removing drv_spi_dma.o(.revsh_text), (4 bytes).
    Removing drv_spi_dma.o(i.__NVIC_ClearPendingIRQ), (24 bytes).
    Removing drv_spi_dma.o(i.drv_spi_abort_dma), (108 bytes).
    Removing drv_spi_dma.o(i.drv_spi_dma_callback), (60 bytes).
    Removing drv_spi_dma.o(i.drv_spi_dma_ch6_init), (208 bytes).
    Removing drv_spi_dma.o(i.drv_spi_dma_init), (220 bytes).
    Removing drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback), (48 bytes).
    Removing drv_spi_dma.o(i.drv_spi_set_dma_irq_callback), (88 bytes).
    Removing drv_spi_dma.o(i.drv_spim_dma_read), (96 bytes).
    Removing drv_spi_dma.o(i.drv_spim_dma_write), (60 bytes).
    Removing drv_spi_dma.o(i.drv_spis_dma_write), (72 bytes).
    Removing drv_spi_dma.o(.bss), (480 bytes).
    Removing drv_spi_dma.o(.data), (16 bytes).
    Removing drv_spi_master.o(.rev16_text), (4 bytes).
    Removing drv_spi_master.o(.revsh_text), (4 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_deinit), (40 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_disable_int), (68 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_enable_int), (72 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_enable_rx_dma), (32 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_enable_tx_dma), (28 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_get_dma_address), (8 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_gpio_init), (32 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_set_intr_callback), (12 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_switch_sclk), (28 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_write_data), (44 bytes).
    Removing drv_spi_master.o(i.drv_spi_master_init), (164 bytes).
    Removing drv_swire.o(.rev16_text), (4 bytes).
    Removing drv_swire.o(.revsh_text), (4 bytes).
    Removing drv_swire.o(i.drv_swire_enable), (28 bytes).
    Removing drv_swire.o(i.drv_swire_register_callback), (12 bytes).
    Removing drv_swire.o(i.drv_swire_set_bit_time), (24 bytes).
    Removing drv_swire.o(i.drv_swire_set_pulse_count), (12 bytes).
    Removing drv_sys_cfg.o(.rev16_text), (4 bytes).
    Removing drv_sys_cfg.o(.revsh_text), (4 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_dma_req_mask), (32 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_read_version0_id), (12 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_set_ap_reset), (28 bytes).
    Removing drv_timer.o(.rev16_text), (4 bytes).
    Removing drv_timer.o(.revsh_text), (4 bytes).
    Removing drv_timer.o(i.drv_timer_get_status), (38 bytes).
    Removing drv_timer.o(i.drv_timer_set_repeat), (16 bytes).
    Removing dcs_packet_fifo.o(i.dcs_packet_get_fifo_size), (16 bytes).
    Removing drv_dsi_rx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_rx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate), (66 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_version), (4 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration), (236 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg), (32 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg), (48 bytes).
    Removing drv_dsi_rx.o(i.drv_rx_phy_test_read), (12 bytes).
    Removing drv_dsi_tx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_tx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_force_interrupt), (8 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_get_phy_status), (6 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_forcepll), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration), (232 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_start), (18 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock), (10 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot), (62 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger), (92 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter), (344 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit), (276 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_sdf_3d), (28 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_bta), (22 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_vpg), (70 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_version), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_vid_shadow), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_read), (10 bytes).
    Removing drv_lcdc.o(.rev16_text), (4 bytes).
    Removing drv_lcdc.o(.revsh_text), (4 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_config_rgb_to_pentile), (6 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_enable), (42 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_update_shadow_reg), (12 bytes).
    Removing drv_memc.o(.rev16_text), (4 bytes).
    Removing drv_memc.o(.revsh_text), (4 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_frm_time), (14 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_int_frame), (28 bytes).
    Removing drv_memc.o(i.drv_memc_set_fb_remaining_line_trigger), (12 bytes).
    Removing drv_memc.o(i.drv_memc_set_read_trigger_line), (16 bytes).
    Removing drv_memc.o(i.drv_memc_set_te_ind), (16 bytes).
    Removing drv_memc.o(i.drv_memc_set_tear_hwclr), (16 bytes).
    Removing drv_memc.o(i.drv_memc_set_vidc_fb_arb), (14 bytes).
    Removing drv_memc.o(i.drv_memc_set_write_trigger_line), (16 bytes).
    Removing drv_rxbr.o(.rev16_text), (4 bytes).
    Removing drv_rxbr.o(.revsh_text), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_dsc_flush), (16 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_cur_hline_rcv_cnt), (8 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_ipi_vsync_interval), (8 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_pix_fmt), (8 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_col_addr), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_compress), (24 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_page_addr), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_soft_reset), (98 bytes).
    Removing drv_vidc.o(.rev16_text), (4 bytes).
    Removing drv_vidc.o(.revsh_text), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_clear_status0), (14 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_cap_pixel), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_signal_frame), (30 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_int_source), (38 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status0), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status1), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status2), (6 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_dsc_thresh), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_frmst_latency), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_inff_thresh), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_irq_line), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_module_enable), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_outff_thresh), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_update_src_format), (14 bytes).
    Removing irq_redirect .o(.rev16_text), (4 bytes).
    Removing irq_redirect .o(.revsh_text), (4 bytes).
    Removing drv_efuse.o(.rev16_text), (4 bytes).
    Removing drv_efuse.o(.revsh_text), (4 bytes).
    Removing drv_efuse.o(i.drv_efuse_crc_cal), (128 bytes).
    Removing drv_efuse.o(i.drv_efuse_get_default_config), (26 bytes).
    Removing drv_efuse.o(i.drv_efuse_int_disable), (12 bytes).
    Removing drv_efuse.o(i.drv_efuse_write), (46 bytes).
    Removing drv_efuse.o(i.drv_efuse_write_req), (22 bytes).
    Removing drv_phy_common.o(.rev16_text), (4 bytes).
    Removing drv_phy_common.o(.revsh_text), (4 bytes).
    Removing drv_phy_common.o(i.drv_phy_test_read), (8 bytes).
    Removing drv_chip_info.o(.rev16_text), (4 bytes).
    Removing drv_chip_info.o(.revsh_text), (4 bytes).
    Removing drv_dsc_dec.o(.rev16_text), (4 bytes).
    Removing drv_dsc_dec.o(.revsh_text), (4 bytes).
    Removing drv_dsc_dec.o(i.drv_dsc_dec_set_u32_pps), (120 bytes).
    Removing tau_log.o(.rev16_text), (4 bytes).
    Removing tau_log.o(.revsh_text), (4 bytes).
    Removing tau_log.o(i.fgetc), (22 bytes).
    Removing app_tp_enc.o(.rev16_text), (4 bytes).
    Removing app_tp_enc.o(.revsh_text), (4 bytes).
    Removing hal_spi_slave.o(.rev16_text), (4 bytes).
    Removing hal_spi_slave.o(.revsh_text), (4 bytes).
    Removing hal_spi_slave.o(i.hal_spi_s_set_high_impedance), (100 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_auto_transfer_abort), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start), (56 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_busy), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_deinit), (10 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_disable), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_enable), (96 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_flush_fifo), (20 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_get_rxfifo_notempty), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_gpio_init), (8 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_init), (76 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_read_data), (10 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_register_callback), (12 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_reset_tx), (68 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_set_auto_rx_buffer), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_set_auto_tx_buffer), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_write_data), (14 bytes).
    Removing norflash.o(.rev16_text), (4 bytes).
    Removing norflash.o(.revsh_text), (4 bytes).
    Removing norflash.o(i.norflash_best_cfg_init), (44 bytes).
    Removing norflash.o(i.norflash_big_end_clear), (14 bytes).
    Removing norflash.o(i.norflash_big_end_enable), (20 bytes).
    Removing norflash.o(i.norflash_check_crc32), (14 bytes).
    Removing norflash.o(i.norflash_check_id), (72 bytes).
    Removing norflash.o(i.norflash_dma_callback), (24 bytes).
    Removing norflash.o(i.norflash_dma_read), (156 bytes).
    Removing norflash.o(i.norflash_dma_write), (252 bytes).
    Removing norflash.o(i.norflash_dual_read), (60 bytes).
    Removing norflash.o(i.norflash_dual_write), (112 bytes).
    Removing norflash.o(i.norflash_en4b), (40 bytes).
    Removing norflash.o(i.norflash_en_quad), (116 bytes).
    Removing norflash.o(i.norflash_en_quad_check), (64 bytes).
    Removing norflash.o(i.norflash_erase_block), (44 bytes).
    Removing norflash.o(i.norflash_erase_chip), (28 bytes).
    Removing norflash.o(i.norflash_erase_sector), (44 bytes).
    Removing norflash.o(i.norflash_ex4b), (40 bytes).
    Removing norflash.o(i.norflash_exit_quad), (76 bytes).
    Removing norflash.o(i.norflash_get_dual_hstatus), (52 bytes).
    Removing norflash.o(i.norflash_get_hstatus), (52 bytes).
    Removing norflash.o(i.norflash_get_status), (52 bytes).
    Removing norflash.o(i.norflash_init), (48 bytes).
    Removing norflash.o(i.norflash_quad_read), (76 bytes).
    Removing norflash.o(i.norflash_quad_write), (108 bytes).
    Removing norflash.o(i.norflash_read), (28 bytes).
    Removing norflash.o(i.norflash_read_config_reg), (36 bytes).
    Removing norflash.o(i.norflash_read_id), (20 bytes).
    Removing norflash.o(i.norflash_read_uid), (52 bytes).
    Removing norflash.o(i.norflash_reset), (2 bytes).
    Removing norflash.o(i.norflash_reset_crc32), (32 bytes).
    Removing norflash.o(i.norflash_set_best_cfg), (50 bytes).
    Removing norflash.o(i.norflash_set_best_read_cfg), (84 bytes).
    Removing norflash.o(i.norflash_set_best_write_cfg), (84 bytes).
    Removing norflash.o(i.norflash_switch_fls_spi), (112 bytes).
    Removing norflash.o(i.norflash_write), (96 bytes).
    Removing norflash.o(i.norflash_write_disable), (64 bytes).
    Removing norflash.o(i.norflash_write_enable), (56 bytes).
    Removing norflash.o(i.norflash_write_endian_scr), (132 bytes).
    Removing norflash.o(.bss), (412 bytes).
    Removing norflash.o(.bss), (32 bytes).
    Removing norflash.o(.data), (2 bytes).
    Removing drv_fls_dma.o(.rev16_text), (4 bytes).
    Removing drv_fls_dma.o(.revsh_text), (4 bytes).
    Removing drv_fls_dma.o(i.fls_abort_dma), (42 bytes).
    Removing drv_fls_dma.o(i.fls_dma_disable), (10 bytes).
    Removing drv_fls_dma.o(i.fls_dma_enable), (10 bytes).
    Removing drv_fls_dma.o(i.fls_dma_read_prepare), (86 bytes).
    Removing drv_fls_dma.o(i.fls_dma_write_prepare), (82 bytes).
    Removing drv_fls_dma.o(i.fls_read_dmacallback), (32 bytes).
    Removing drv_fls_dma.o(i.fls_transfer_create_handle_dma), (208 bytes).
    Removing drv_fls_dma.o(i.fls_transfer_dma), (112 bytes).
    Removing drv_fls_dma.o(i.fls_transfer_get_receive_count_dma), (44 bytes).
    Removing drv_fls_dma.o(i.fls_write_dmacallback), (32 bytes).
    Removing drv_fls_dma.o(.data), (8 bytes).
    Removing drv_pwm.o(.rev16_text), (4 bytes).
    Removing drv_pwm.o(.revsh_text), (4 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_clear_pwm_int_all), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_enable), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_counter_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_current_count), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_high_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_low_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_register_callback), (24 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_set_pwm_int), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_set_sys_int), (64 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_enable), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_get_sync_flag), (16 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_pause), (28 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_control), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_sync_mode), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_threshold), (12 bytes).
    Removing drv_spi_slave.o(.rev16_text), (4 bytes).
    Removing drv_spi_slave.o(.revsh_text), (4 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_deinit), (40 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_disable_int), (68 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_enable_int), (72 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_enable_rx_dma), (32 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_enable_tx_dma), (28 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_get_dma_address), (8 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_gpio_init), (24 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_read_data), (32 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_switch_sclk), (28 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_write_data), (44 bytes).
    Removing drv_spi_slave.o(i.drv_spi_slave_init), (76 bytes).
    Removing drv_uart.o(.rev16_text), (4 bytes).
    Removing drv_uart.o(.revsh_text), (4 bytes).
    Removing drv_uart.o(i.UART_AbortReceive), (30 bytes).
    Removing drv_uart.o(i.UART_AbortSend), (30 bytes).
    Removing drv_uart.o(i.UART_Deinit), (28 bytes).
    Removing drv_uart.o(i.UART_Disable_IT), (68 bytes).
    Removing drv_uart.o(i.UART_EnableDma), (32 bytes).
    Removing drv_uart.o(i.UART_Enable_IT), (44 bytes).
    Removing drv_uart.o(i.UART_GetDefaultConfig), (72 bytes).
    Removing drv_uart.o(i.UART_GetFIFO_Ctrl), (20 bytes).
    Removing drv_uart.o(i.UART_GetReceiveCount), (22 bytes).
    Removing drv_uart.o(i.UART_GetReceiveStatus), (20 bytes).
    Removing drv_uart.o(i.UART_GetRxRingBufferLength), (28 bytes).
    Removing drv_uart.o(i.UART_GetSendCount), (22 bytes).
    Removing drv_uart.o(i.UART_GetSendStatus), (20 bytes).
    Removing drv_uart.o(i.UART_ReadBlocking), (32 bytes).
    Removing drv_uart.o(i.UART_ReceiveNonBlocking), (50 bytes).
    Removing drv_uart.o(i.UART_ResetTxFIFO), (36 bytes).
    Removing drv_uart.o(i.UART_SendNonBlocking), (38 bytes).
    Removing drv_uart.o(i.UART_TransferCreateHandle), (96 bytes).
    Removing drv_uart.o(i.UART_TransferStartRingBuffer), (30 bytes).
    Removing drv_uart.o(.constdata), (1 bytes).
    Removing drv_uart_dma.o(.rev16_text), (4 bytes).
    Removing drv_uart_dma.o(.revsh_text), (4 bytes).
    Removing drv_uart_dma.o(i.UART_DMAInit), (76 bytes).
    Removing drv_uart_dma.o(i.UART_TransferAbortReceiveDMA), (16 bytes).
    Removing drv_uart_dma.o(i.UART_TransferAbortSendDMA), (16 bytes).
    Removing drv_uart_dma.o(i.UART_TransferCreateHandleDMA), (176 bytes).
    Removing drv_uart_dma.o(i.UART_TransferGetReceiveCountDMA), (44 bytes).
    Removing drv_uart_dma.o(i.UART_TransferReceiveDMA), (68 bytes).
    Removing drv_uart_dma.o(i.UART_TransferReceiveDMACallback), (34 bytes).
    Removing drv_uart_dma.o(i.UART_TransferSendDMA), (68 bytes).
    Removing drv_uart_dma.o(i.UART_TransferSendDMACallback), (34 bytes).
    Removing drv_uart_dma.o(.data), (8 bytes).
    Removing drv_wdg.o(.rev16_text), (4 bytes).
    Removing drv_wdg.o(.revsh_text), (4 bytes).
    Removing drv_wdg.o(i.drv_wdg_enable), (32 bytes).
    Removing drv_wdg.o(i.drv_wdg_load_match), (12 bytes).
    Removing drv_wdg.o(i.drv_wdg_register_callback), (12 bytes).
    Removing drv_wdg.o(i.drv_wdg_sel_mode), (28 bytes).
    Removing drv_wdg.o(i.drv_wdg_set_repeat), (12 bytes).
    Removing dflti.o(.text), (40 bytes).

586 unused section(s) (total 26778 bytes) removed from the image.

==============================================================================

Image Symbol Table

    Local Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    ../clib/../cmprslib/zerorunl2.c          0x00000000   Number         0  __dczerorl2.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  idiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uidiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uldiv.o ABSOLUTE
    ../clib/microlib/errno.c                 0x00000000   Number         0  errno.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry2.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry5.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llshl.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llushr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llsshr.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf7.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf8.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfa.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf4.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf3.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf1.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf2.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf0.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfb.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf5.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf6.o ABSOLUTE
    ../clib/microlib/printf/stubs.s          0x00000000   Number         0  stubs.o ABSOLUTE
    ../clib/microlib/stdio/streams.c         0x00000000   Number         0  stdout.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpyb.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpya.o ABSOLUTE
    ../clib/microlib/string/memset.c         0x00000000   Number         0  memseta.o ABSOLUTE
    ../clib/microlib/stubs.s                 0x00000000   Number         0  iusefp.o ABSOLUTE
    ../fplib/microlib/f2d.c                  0x00000000   Number         0  f2d.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  fadd.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  dadd.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  fdiv.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  ddiv.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  depilogue.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  fepilogue.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  ffixui.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixui.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixi.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  ffixi.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixul.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  dflti.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  ffltui.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  fflti.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  dfltui.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  fmul.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  dmul.o ABSOLUTE
    ../fplib/microlib/fpscalb.c              0x00000000   Number         0  fscalb.o ABSOLUTE
    ../fplib/microlib/fpsqrt.c               0x00000000   Number         0  dsqrt.o ABSOLUTE
    ../mathlib/ceil.c                        0x00000000   Number         0  ceil.o ABSOLUTE
    ../mathlib/sqrt.c                        0x00000000   Number         0  sqrt.o ABSOLUTE
    ../mathlib/sqrt.c                        0x00000000   Number         0  sqrt_x.o ABSOLUTE
    ..\..\..\src\common\tau_delay.c          0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\..\..\src\common\tau_log.c            0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\..\..\src\driver\robin\src\drv_chip_info.c 0x00000000   Number         0  drv_chip_info.o ABSOLUTE
    ..\..\..\src\driver\robin\src\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\irq_redirect .c 0x00000000   Number         0  irq_redirect .o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\internal\dcs_packet_fifo.c 0x00000000   Number         0  dcs_packet_fifo.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_fls.c 0x00000000   Number         0  drv_fls.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_fls_dma.c 0x00000000   Number         0  drv_fls_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_i2c_dma.c 0x00000000   Number         0  drv_i2c_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_i2c_master.c 0x00000000   Number         0  drv_i2c_master.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_i2c_slave.c 0x00000000   Number         0  drv_i2c_slave.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_param_init.c 0x00000000   Number         0  drv_param_init.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_pwm.c 0x00000000   Number         0  drv_pwm.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_spi_dma.c 0x00000000   Number         0  drv_spi_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_spi_master.c 0x00000000   Number         0  drv_spi_master.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_spi_slave.c 0x00000000   Number         0  drv_spi_slave.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_uart_dma.c 0x00000000   Number         0  drv_uart_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_wdg.c 0x00000000   Number         0  drv_wdg.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_i2c_master.c 0x00000000   Number         0  hal_i2c_master.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_i2c_slave.c 0x00000000   Number         0  hal_i2c_slave.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_spi_master.c 0x00000000   Number         0  hal_spi_master.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_spi_slave.c 0x00000000   Number         0  hal_spi_slave.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_swire.c 0x00000000   Number         0  hal_swire.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_timer.c 0x00000000   Number         0  hal_timer.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\internal\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\internal\norflash.c 0x00000000   Number         0  norflash.o ABSOLUTE
    ..\..\src\app\ap_demo\app_tp_enc.c       0x00000000   Number         0  app_tp_enc.o ABSOLUTE
    ..\..\src\app\demo\ap_demo.c             0x00000000   Number         0  ap_demo.o ABSOLUTE
    ..\..\src\app\demo\app_tp_for_custom_s8.c 0x00000000   Number         0  app_tp_for_custom_s8.o ABSOLUTE
    ..\..\src\app\demo\app_tp_st_touch.c     0x00000000   Number         0  app_tp_st_touch.o ABSOLUTE
    ..\..\src\app\demo\app_tp_transfer.c     0x00000000   Number         0  app_tp_transfer.o ABSOLUTE
    ..\..\src\app\main.c                     0x00000000   Number         0  main.o ABSOLUTE
    ..\..\src\board\board.c                  0x00000000   Number         0  board.o ABSOLUTE
    ..\..\src\board\startup\startup_ARMCM0.s 0x00000000   Number         0  startup_armcm0.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_delay.c     0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_log.c       0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\\..\\..\\src\\driver\\robin\\src\\drv_chip_info.c 0x00000000   Number         0  drv_chip_info.o ABSOLUTE
    ..\\..\\..\\src\\driver\\robin\\src\\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\irq_redirect .c 0x00000000   Number         0  irq_redirect .o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_fls.c 0x00000000   Number         0  drv_fls.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_fls_dma.c 0x00000000   Number         0  drv_fls_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_i2c_dma.c 0x00000000   Number         0  drv_i2c_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_i2c_master.c 0x00000000   Number         0  drv_i2c_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_i2c_slave.c 0x00000000   Number         0  drv_i2c_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_param_init.c 0x00000000   Number         0  drv_param_init.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_pwm.c 0x00000000   Number         0  drv_pwm.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_spi_dma.c 0x00000000   Number         0  drv_spi_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_spi_master.c 0x00000000   Number         0  drv_spi_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_spi_slave.c 0x00000000   Number         0  drv_spi_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_uart_dma.c 0x00000000   Number         0  drv_uart_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_wdg.c 0x00000000   Number         0  drv_wdg.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_i2c_master.c 0x00000000   Number         0  hal_i2c_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_i2c_slave.c 0x00000000   Number         0  hal_i2c_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_spi_master.c 0x00000000   Number         0  hal_spi_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_spi_slave.c 0x00000000   Number         0  hal_spi_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_swire.c 0x00000000   Number         0  hal_swire.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_timer.c 0x00000000   Number         0  hal_timer.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\internal\\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\internal\\norflash.c 0x00000000   Number         0  norflash.o ABSOLUTE
    ..\\..\\src\\app\\ap_demo\\app_tp_enc.c  0x00000000   Number         0  app_tp_enc.o ABSOLUTE
    ..\\..\\src\\app\\demo\\ap_demo.c        0x00000000   Number         0  ap_demo.o ABSOLUTE
    ..\\..\\src\\app\\demo\\app_tp_for_custom_s8.c 0x00000000   Number         0  app_tp_for_custom_s8.o ABSOLUTE
    ..\\..\\src\\app\\demo\\app_tp_st_touch.c 0x00000000   Number         0  app_tp_st_touch.o ABSOLUTE
    ..\\..\\src\\app\\demo\\app_tp_transfer.c 0x00000000   Number         0  app_tp_transfer.o ABSOLUTE
    ..\\..\\src\\app\\main.c                 0x00000000   Number         0  main.o ABSOLUTE
    ..\\..\\src\\board\\board.c              0x00000000   Number         0  board.o ABSOLUTE
    cdcmple.s                                0x00000000   Number         0  cdcmple.o ABSOLUTE
    cdrcmple.s                               0x00000000   Number         0  cdrcmple.o ABSOLUTE
    cfrcmple.s                               0x00000000   Number         0  cfrcmple.o ABSOLUTE
    dc.s                                     0x00000000   Number         0  dc.o ABSOLUTE
    handlers.s                               0x00000000   Number         0  handlers.o ABSOLUTE
    init.s                                   0x00000000   Number         0  init.o ABSOLUTE
    RESET                                    0x00010000   Section      192  startup_armcm0.o(RESET)
    .ARM.Collect$$$$00000000                 0x000100c0   Section        0  entry.o(.ARM.Collect$$$$00000000)
    .ARM.Collect$$$$00000001                 0x000100c0   Section        4  entry2.o(.ARM.Collect$$$$00000001)
    .ARM.Collect$$$$00000004                 0x000100c4   Section        4  entry5.o(.ARM.Collect$$$$00000004)
    .ARM.Collect$$$$00000008                 0x000100c8   Section        0  entry7b.o(.ARM.Collect$$$$00000008)
    .ARM.Collect$$$$0000000A                 0x000100c8   Section        0  entry8b.o(.ARM.Collect$$$$0000000A)
    .ARM.Collect$$$$0000000B                 0x000100c8   Section        8  entry9a.o(.ARM.Collect$$$$0000000B)
    .ARM.Collect$$$$0000000D                 0x000100d0   Section        0  entry10a.o(.ARM.Collect$$$$0000000D)
    .ARM.Collect$$$$0000000F                 0x000100d0   Section        0  entry11a.o(.ARM.Collect$$$$0000000F)
    .ARM.Collect$$$$00002712                 0x000100d0   Section        4  entry2.o(.ARM.Collect$$$$00002712)
    __lit__00000000                          0x000100d0   Data           4  entry2.o(.ARM.Collect$$$$00002712)
    .text                                    0x000100d4   Section      120  startup_armcm0.o(.text)
    .text                                    0x0001014c   Section        0  uidiv.o(.text)
    .text                                    0x00010178   Section        0  idiv.o(.text)
    .text                                    0x000101a0   Section        0  memcpya.o(.text)
    .text                                    0x000101c4   Section        0  memseta.o(.text)
    .text                                    0x000101e8   Section        0  fadd.o(.text)
    .text                                    0x0001029a   Section        0  fmul.o(.text)
    .text                                    0x00010314   Section        0  fdiv.o(.text)
    .text                                    0x00010390   Section        0  fscalb.o(.text)
    .text                                    0x000103a8   Section        0  dadd.o(.text)
    .text                                    0x0001050c   Section        0  dmul.o(.text)
    .text                                    0x000105dc   Section        0  ddiv.o(.text)
    .text                                    0x000106cc   Section        0  fflti.o(.text)
    .text                                    0x000106e2   Section        0  ffltui.o(.text)
    .text                                    0x000106f0   Section        0  dfltui.o(.text)
    .text                                    0x0001070c   Section        0  ffixi.o(.text)
    .text                                    0x0001073e   Section        0  ffixui.o(.text)
    .text                                    0x00010768   Section        0  dfixi.o(.text)
    .text                                    0x000107b0   Section        0  dfixui.o(.text)
    .text                                    0x000107ec   Section        0  f2d.o(.text)
    .text                                    0x00010814   Section       40  cdcmple.o(.text)
    .text                                    0x0001083c   Section       20  cfrcmple.o(.text)
    .text                                    0x00010850   Section        0  uldiv.o(.text)
    .text                                    0x000108b0   Section        0  llshl.o(.text)
    .text                                    0x000108d0   Section        0  llushr.o(.text)
    .text                                    0x000108f2   Section        0  llsshr.o(.text)
    .text                                    0x00010918   Section        0  fepilogue.o(.text)
    .text                                    0x00010918   Section        0  iusefp.o(.text)
    .text                                    0x0001099a   Section        0  depilogue.o(.text)
    .text                                    0x00010a58   Section        0  dsqrt.o(.text)
    .text                                    0x00010afc   Section        0  dfixul.o(.text)
    .text                                    0x00010b3c   Section       40  cdrcmple.o(.text)
    .text                                    0x00010b64   Section       36  init.o(.text)
    .text                                    0x00010b88   Section        0  __dczerorl2.o(.text)
    i.ADC_IRQn_Handler                       0x00010be0   Section        0  irq_redirect .o(i.ADC_IRQn_Handler)
    i.AP_NRESET_IRQn_Handler                 0x00010bf8   Section        0  irq_redirect .o(i.AP_NRESET_IRQn_Handler)
    i.DMA_IRQn_Handler                       0x00010c10   Section        0  irq_redirect .o(i.DMA_IRQn_Handler)
    i.EXTI_INT0_IRQn_Handler                 0x00010c24   Section        0  irq_redirect .o(i.EXTI_INT0_IRQn_Handler)
    i.EXTI_INT1_IRQn_Handler                 0x00010c40   Section        0  irq_redirect .o(i.EXTI_INT1_IRQn_Handler)
    i.EXTI_INT2_IRQn_Handler                 0x00010c5c   Section        0  irq_redirect .o(i.EXTI_INT2_IRQn_Handler)
    i.EXTI_INT3_IRQn_Handler                 0x00010c78   Section        0  irq_redirect .o(i.EXTI_INT3_IRQn_Handler)
    i.EXTI_INT4_IRQn_Handler                 0x00010c94   Section        0  irq_redirect .o(i.EXTI_INT4_IRQn_Handler)
    i.EXTI_INT5_IRQn_Handler                 0x00010cb0   Section        0  irq_redirect .o(i.EXTI_INT5_IRQn_Handler)
    i.EXTI_INT6_IRQn_Handler                 0x00010ccc   Section        0  irq_redirect .o(i.EXTI_INT6_IRQn_Handler)
    i.EXTI_INT7_IRQn_Handler                 0x00010ce8   Section        0  irq_redirect .o(i.EXTI_INT7_IRQn_Handler)
    i.EncryptCheck                           0x00010d04   Section        0  app_tp_enc.o(i.EncryptCheck)
    i.FLSCTRL_IRQn_Handler                   0x00010d68   Section        0  irq_redirect .o(i.FLSCTRL_IRQn_Handler)
    i.Gpio_swire_output                      0x00010d7c   Section        0  ap_demo.o(i.Gpio_swire_output)
    i.HardFault_Handler                      0x00010df0   Section        0  irq_redirect .o(i.HardFault_Handler)
    i.I2C0_IRQn_Handler                      0x00010e04   Section        0  irq_redirect .o(i.I2C0_IRQn_Handler)
    i.I2C1_IRQn_Handler                      0x00010e1c   Section        0  irq_redirect .o(i.I2C1_IRQn_Handler)
    i.LCDC_IRQn_Handler                      0x00010e34   Section        0  irq_redirect .o(i.LCDC_IRQn_Handler)
    i.LOG_printf                             0x00010e4c   Section        0  tau_log.o(i.LOG_printf)
    i.MEMC_IRQn_Handler                      0x00010e74   Section        0  irq_redirect .o(i.MEMC_IRQn_Handler)
    i.MIPI_RX_IRQn_Handler                   0x00010e8c   Section        0  irq_redirect .o(i.MIPI_RX_IRQn_Handler)
    i.MIPI_TX_IRQn_Handler                   0x00010ea4   Section        0  irq_redirect .o(i.MIPI_TX_IRQn_Handler)
    i.PWMDET_IRQn_Handler                    0x00010ebc   Section        0  irq_redirect .o(i.PWMDET_IRQn_Handler)
    i.SPIM_IRQn_Handler                      0x00010ed8   Section        0  irq_redirect .o(i.SPIM_IRQn_Handler)
    i.SPIS_IRQn_Handler                      0x00010ef4   Section        0  irq_redirect .o(i.SPIS_IRQn_Handler)
    i.SWIRE_IRQn_Handler                     0x00010f10   Section        0  irq_redirect .o(i.SWIRE_IRQn_Handler)
    i.SysTick_Handler                        0x00010f2c   Section        0  irq_redirect .o(i.SysTick_Handler)
    i.TIMER0_IRQn_Handler                    0x00010f44   Section        0  irq_redirect .o(i.TIMER0_IRQn_Handler)
    i.TIMER1_IRQn_Handler                    0x00010f5c   Section        0  irq_redirect .o(i.TIMER1_IRQn_Handler)
    i.TIMER2_IRQn_Handler                    0x00010f74   Section        0  irq_redirect .o(i.TIMER2_IRQn_Handler)
    i.TIMER3_IRQn_Handler                    0x00010f8c   Section        0  irq_redirect .o(i.TIMER3_IRQn_Handler)
    i.UART0_IRQ_Handle                       0x00010fa4   Section        0  drv_uart.o(i.UART0_IRQ_Handle)
    i.UART_DisableDma                        0x00010fc0   Section        0  drv_uart.o(i.UART_DisableDma)
    i.UART_GetInstance                       0x00010fc2   Section        0  drv_uart.o(i.UART_GetInstance)
    i.UART_IRQn_Handler                      0x00010fc8   Section        0  irq_redirect .o(i.UART_IRQn_Handler)
    i.UART_SwitchSCLK                        0x00010fe0   Section        0  drv_uart.o(i.UART_SwitchSCLK)
    i.__scatterload_null                     0x00010ffa   Section        2  handlers.o(i.__scatterload_null)
    i.drv_dsi_rx_set_inten                   0x00010ffc   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    .ARM.__at_0x11000                        0x00011000   Section       20  drv_common.o(.ARM.__at_0x11000)
    i.drv_dsi_tx_command_put_payload         0x00011014   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    .ARM.__at_0x11018                        0x00011018   Section        4  drv_common.o(.ARM.__at_0x11018)
    i.S20_Start_init                         0x0001101c   Section        0  app_tp_transfer.o(i.S20_Start_init)
    i.UART_ResetRxFIFO                       0x00011160   Section        0  drv_uart.o(i.UART_ResetRxFIFO)
    i.UART_SetBaudRate                       0x00011184   Section        0  drv_uart.o(i.UART_SetBaudRate)
    i.UART_TransferHandleIRQ                 0x000111cc   Section        0  drv_uart.o(i.UART_TransferHandleIRQ)
    i.UART_WriteBlocking                     0x00011300   Section        0  drv_uart.o(i.UART_WriteBlocking)
    i.UART_init                              0x0001131c   Section        0  drv_uart.o(i.UART_init)
    i.VIDC_IRQn_Handler                      0x000113d8   Section        0  irq_redirect .o(i.VIDC_IRQn_Handler)
    i.VPRE_IRQn_Handler                      0x000113f0   Section        0  irq_redirect .o(i.VPRE_IRQn_Handler)
    i.WDG_IRQn_Handler                       0x00011408   Section        0  irq_redirect .o(i.WDG_IRQn_Handler)
    i.__0printf                              0x00011420   Section        0  printfa.o(i.__0printf)
    i.__0vsprintf                            0x00011440   Section        0  printfa.o(i.__0vsprintf)
    i.__ARM_clz                              0x00011464   Section        0  depilogue.o(i.__ARM_clz)
    i.__ARM_common_switch8                   0x00011492   Section        0  ap_demo.o(i.__ARM_common_switch8)
    i.__NVIC_ClearPendingIRQ                 0x000114ac   Section        0  drv_i2c_master.o(i.__NVIC_ClearPendingIRQ)
    __NVIC_ClearPendingIRQ                   0x000114ad   Thumb Code    18  drv_i2c_master.o(i.__NVIC_ClearPendingIRQ)
    i.__NVIC_ClearPendingIRQ                 0x000114c4   Section        0  drv_spi_master.o(i.__NVIC_ClearPendingIRQ)
    __NVIC_ClearPendingIRQ                   0x000114c5   Thumb Code    18  drv_spi_master.o(i.__NVIC_ClearPendingIRQ)
    i.__NVIC_DisableIRQ                      0x000114dc   Section        0  drv_rxbr.o(i.__NVIC_DisableIRQ)
    __NVIC_DisableIRQ                        0x000114dd   Thumb Code    26  drv_rxbr.o(i.__NVIC_DisableIRQ)
    i.__NVIC_EnableIRQ                       0x000114fc   Section        0  drv_rxbr.o(i.__NVIC_EnableIRQ)
    __NVIC_EnableIRQ                         0x000114fd   Thumb Code    18  drv_rxbr.o(i.__NVIC_EnableIRQ)
    i.__NVIC_SetPriority                     0x00011514   Section        0  hal_spi_slave.o(i.__NVIC_SetPriority)
    __NVIC_SetPriority                       0x00011515   Thumb Code    60  hal_spi_slave.o(i.__NVIC_SetPriority)
    i.__scatterload_copy                     0x00011558   Section       14  handlers.o(i.__scatterload_copy)
    i.__scatterload_zeroinit                 0x00011566   Section       14  handlers.o(i.__scatterload_zeroinit)
    i.__set_errno                            0x00011574   Section        0  errno.o(i.__set_errno)
    i._fp_digits                             0x00011580   Section        0  printfa.o(i._fp_digits)
    _fp_digits                               0x00011581   Thumb Code   344  printfa.o(i._fp_digits)
    i._printf_core                           0x000116f4   Section        0  printfa.o(i._printf_core)
    _printf_core                             0x000116f5   Thumb Code  1754  printfa.o(i._printf_core)
    i._printf_post_padding                   0x00011de0   Section        0  printfa.o(i._printf_post_padding)
    _printf_post_padding                     0x00011de1   Thumb Code    32  printfa.o(i._printf_post_padding)
    i._printf_pre_padding                    0x00011e00   Section        0  printfa.o(i._printf_pre_padding)
    _printf_pre_padding                      0x00011e01   Thumb Code    44  printfa.o(i._printf_pre_padding)
    i._sputc                                 0x00011e2c   Section        0  printfa.o(i._sputc)
    _sputc                                   0x00011e2d   Thumb Code    10  printfa.o(i._sputc)
    i.ap_dcs_read                            0x00011e38   Section        0  ap_demo.o(i.ap_dcs_read)
    ap_dcs_read                              0x00011e39   Thumb Code  4188  ap_demo.o(i.ap_dcs_read)
    i.ap_demo                                0x00012e94   Section        0  ap_demo.o(i.ap_demo)
    i.ap_get_reg_ca                          0x00012fcc   Section        0  ap_demo.o(i.ap_get_reg_ca)
    ap_get_reg_ca                            0x00012fcd   Thumb Code    36  ap_demo.o(i.ap_get_reg_ca)
    i.ap_get_reg_df                          0x00012ff4   Section        0  ap_demo.o(i.ap_get_reg_df)
    ap_get_reg_df                            0x00012ff5   Thumb Code   170  ap_demo.o(i.ap_get_reg_df)
    i.ap_get_tp_calibration_status_01        0x000130a4   Section        0  app_tp_st_touch.o(i.ap_get_tp_calibration_status_01)
    i.ap_reset_cb                            0x000130c4   Section        0  ap_demo.o(i.ap_reset_cb)
    ap_reset_cb                              0x000130c5   Thumb Code    30  ap_demo.o(i.ap_reset_cb)
    i.ap_set_backlight                       0x000130ec   Section        0  ap_demo.o(i.ap_set_backlight)
    ap_set_backlight                         0x000130ed   Thumb Code   672  ap_demo.o(i.ap_set_backlight)
    i.ap_set_display_off                     0x000133ac   Section        0  ap_demo.o(i.ap_set_display_off)
    ap_set_display_off                       0x000133ad   Thumb Code    32  ap_demo.o(i.ap_set_display_off)
    i.ap_set_display_on                      0x000133d0   Section        0  ap_demo.o(i.ap_set_display_on)
    ap_set_display_on                        0x000133d1   Thumb Code     8  ap_demo.o(i.ap_set_display_on)
    i.ap_set_enter_sleep_mode                0x000133dc   Section        0  ap_demo.o(i.ap_set_enter_sleep_mode)
    ap_set_enter_sleep_mode                  0x000133dd   Thumb Code    46  ap_demo.o(i.ap_set_enter_sleep_mode)
    i.ap_set_exit_sleep_mode                 0x00013414   Section        0  ap_demo.o(i.ap_set_exit_sleep_mode)
    ap_set_exit_sleep_mode                   0x00013415   Thumb Code     8  ap_demo.o(i.ap_set_exit_sleep_mode)
    i.ap_set_tp_calibration_04               0x00013420   Section        0  ap_demo.o(i.ap_set_tp_calibration_04)
    ap_set_tp_calibration_04                 0x00013421   Thumb Code    22  ap_demo.o(i.ap_set_tp_calibration_04)
    i.ap_tp_st_touch_calibration             0x0001343c   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_calibration)
    i.ap_tp_st_touch_error_handler_F3        0x000134ec   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_F3)
    i.ap_tp_st_touch_error_handler_FF        0x00013506   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_FF)
    i.ap_tp_st_touch_get_calibration_success_mark 0x00013528   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark)
    i.ap_tp_st_touch_scan_point_init         0x000135d0   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init)
    i.ap_tp_st_touch_scan_point_record_event 0x000135ec   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event)
    i.ap_tp_st_touch_scan_point_record_event_exec 0x00013680   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec)
    i.ap_tp_st_touch_simulate_finger_release_event 0x000136b4   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event)
    i.ap_tp_st_touch_software_reset          0x000136e8   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_software_reset)
    i.ap_update_frame_rate                   0x00013758   Section        0  ap_demo.o(i.ap_update_frame_rate)
    ap_update_frame_rate                     0x00013759   Thumb Code    40  ap_demo.o(i.ap_update_frame_rate)
    i.app_ADC_IRQn_Handler                   0x00013784   Section        0  drv_rxbr.o(i.app_ADC_IRQn_Handler)
    i.app_AP_NRESET_IRQn_Handler             0x000137a0   Section        0  drv_gpio.o(i.app_AP_NRESET_IRQn_Handler)
    i.app_EXTI_INT0_IRQn_Handler             0x000137c4   Section        0  drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler)
    i.app_EXTI_INT1_IRQn_Handler             0x000137e0   Section        0  drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler)
    i.app_EXTI_INT2_IRQn_Handler             0x000137fc   Section        0  drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler)
    i.app_EXTI_INT3_IRQn_Handler             0x00013818   Section        0  drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler)
    i.app_EXTI_INT4_IRQn_Handler             0x00013834   Section        0  drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler)
    i.app_EXTI_INT5_IRQn_Handler             0x00013850   Section        0  drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler)
    i.app_EXTI_INT6_IRQn_Handler             0x0001386c   Section        0  drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler)
    i.app_EXTI_INT7_IRQn_Handler             0x00013888   Section        0  drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler)
    i.app_HardFault_Handler                  0x000138a4   Section        0  drv_common.o(i.app_HardFault_Handler)
    i.app_I2C0_IRQn_Handler                  0x000138ec   Section        0  drv_i2c_slave.o(i.app_I2C0_IRQn_Handler)
    i.app_I2C1_IRQn_Handler                  0x00013904   Section        0  drv_i2c_master.o(i.app_I2C1_IRQn_Handler)
    i.app_LCDC_IRQn_Handler                  0x00013914   Section        0  hal_internal_vsync.o(i.app_LCDC_IRQn_Handler)
    i.app_MEMC_IRQn_Handler                  0x00013ab8   Section        0  drv_memc.o(i.app_MEMC_IRQn_Handler)
    i.app_MIPI_RX_IRQn_Handler               0x00013b40   Section        0  drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler)
    i.app_MIPI_TX_IRQn_Handler               0x00013dd8   Section        0  drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler)
    i.app_PWMDET_IRQn_Handler                0x00013e78   Section        0  drv_pwm.o(i.app_PWMDET_IRQn_Handler)
    i.app_SPIM_IRQn_Handler                  0x00013ec0   Section        0  drv_spi_master.o(i.app_SPIM_IRQn_Handler)
    i.app_SPIS_IRQn_Handler                  0x00013ef0   Section        0  hal_spi_slave.o(i.app_SPIS_IRQn_Handler)
    i.app_SWIRE_IRQn_Handler                 0x000140f0   Section        0  drv_swire.o(i.app_SWIRE_IRQn_Handler)
    i.app_SysTick_Handler                    0x00014110   Section        0  drv_common.o(i.app_SysTick_Handler)
    i.app_TIMER0_IRQn_Handler                0x00014128   Section        0  drv_timer.o(i.app_TIMER0_IRQn_Handler)
    i.app_TIMER1_IRQn_Handler                0x00014132   Section        0  drv_timer.o(i.app_TIMER1_IRQn_Handler)
    i.app_TIMER2_IRQn_Handler                0x0001413c   Section        0  drv_timer.o(i.app_TIMER2_IRQn_Handler)
    i.app_TIMER3_IRQn_Handler                0x00014146   Section        0  drv_timer.o(i.app_TIMER3_IRQn_Handler)
    i.app_UART_IRQn_Handler                  0x00014150   Section        0  drv_uart.o(i.app_UART_IRQn_Handler)
    i.app_VIDC_IRQn_Handler                  0x00014158   Section        0  drv_vidc.o(i.app_VIDC_IRQn_Handler)
    i.app_VPRE_IRQn_Handler                  0x00014174   Section        0  drv_rxbr.o(i.app_VPRE_IRQn_Handler)
    i.app_WDG_IRQn_Handler                   0x00014190   Section        0  drv_wdg.o(i.app_WDG_IRQn_Handler)
    i.app_dma_irq_handler                    0x000141c8   Section        0  drv_dma.o(i.app_dma_irq_handler)
    i.app_fls_ctrl_Handler                   0x000141d8   Section        0  norflash.o(i.app_fls_ctrl_Handler)
    i.app_tp_I2C_init                        0x00014208   Section        0  app_tp_transfer.o(i.app_tp_I2C_init)
    i.app_tp_calibration_exec                0x0001422c   Section        0  app_tp_st_touch.o(i.app_tp_calibration_exec)
    i.app_tp_i2cs_callback                   0x00014264   Section        0  app_tp_transfer.o(i.app_tp_i2cs_callback)
    app_tp_i2cs_callback                     0x00014265   Thumb Code    42  app_tp_transfer.o(i.app_tp_i2cs_callback)
    i.app_tp_init                            0x00014294   Section        0  app_tp_transfer.o(i.app_tp_init)
    i.app_tp_m_read                          0x000142d8   Section        0  app_tp_transfer.o(i.app_tp_m_read)
    i.app_tp_m_write                         0x000142f8   Section        0  app_tp_transfer.o(i.app_tp_m_write)
    i.app_tp_phone_analysis_data             0x00014300   Section        0  app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data)
    i.app_tp_phone_clear_reset_on            0x0001471c   Section        0  app_tp_transfer.o(i.app_tp_phone_clear_reset_on)
    i.app_tp_s_read                          0x00014728   Section        0  app_tp_transfer.o(i.app_tp_s_read)
    i.app_tp_s_write                         0x00014730   Section        0  app_tp_transfer.o(i.app_tp_s_write)
    i.app_tp_screen_analysis_int             0x00014738   Section        0  app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int)
    i.app_tp_screen_init                     0x00014a14   Section        0  app_tp_transfer.o(i.app_tp_screen_init)
    i.app_tp_screen_int_callback             0x00014a44   Section        0  app_tp_transfer.o(i.app_tp_screen_int_callback)
    app_tp_screen_int_callback               0x00014a45   Thumb Code     8  app_tp_transfer.o(i.app_tp_screen_int_callback)
    i.app_tp_transfer_screen_const           0x00014a50   Section        0  app_tp_transfer.o(i.app_tp_transfer_screen_const)
    app_tp_transfer_screen_const             0x00014a51   Thumb Code    50  app_tp_transfer.o(i.app_tp_transfer_screen_const)
    i.app_tp_transfer_screen_int             0x00014a90   Section        0  app_tp_transfer.o(i.app_tp_transfer_screen_int)
    i.app_tp_transfer_screen_start           0x00014bf0   Section        0  app_tp_transfer.o(i.app_tp_transfer_screen_start)
    i.blue_change_ccm                        0x00014c08   Section        0  ap_demo.o(i.blue_change_ccm)
    i.board_Init                             0x00014c40   Section        0  board.o(i.board_Init)
    i.calc_framebuffer_setting               0x00014c64   Section        0  hal_internal_vsync.o(i.calc_framebuffer_setting)
    i.ceil                                   0x00015154   Section        0  ceil.o(i.ceil)
    i.check_mipi_rx_tx_video_info            0x0001521c   Section        0  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    check_mipi_rx_tx_video_info              0x0001521d   Thumb Code    44  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    i.check_pkt_buf_rev                      0x00015248   Section        0  hal_internal_vsync.o(i.check_pkt_buf_rev)
    check_pkt_buf_rev                        0x00015249   Thumb Code    92  hal_internal_vsync.o(i.check_pkt_buf_rev)
    i.dcs_packet_fifo_alloc                  0x000152d8   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    i.dcs_packet_fifo_init                   0x00015330   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    i.dcs_packet_free_fifo_header            0x00015348   Section        0  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    i.dcs_packet_get_fifo_header             0x0001538c   Section        0  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    i.dcs_sw_filter                          0x000153b0   Section        0  hal_internal_vsync.o(i.dcs_sw_filter)
    dcs_sw_filter                            0x000153b1   Thumb Code    36  hal_internal_vsync.o(i.dcs_sw_filter)
    i.delayMs                                0x000153dc   Section        0  tau_delay.o(i.delayMs)
    i.delayUs                                0x000153f4   Section        0  tau_delay.o(i.delayUs)
    i.disable_mipi_timer_cb                  0x00015418   Section        0  ap_demo.o(i.disable_mipi_timer_cb)
    disable_mipi_timer_cb                    0x00015419   Thumb Code    78  ap_demo.o(i.disable_mipi_timer_cb)
    i.drv_ap_rst_trig_edge_detect            0x00015470   Section        0  drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect)
    i.drv_chip_info_get_info                 0x000154a8   Section        0  drv_chip_info.o(i.drv_chip_info_get_info)
    i.drv_chip_info_init                     0x000154b4   Section        0  drv_chip_info.o(i.drv_chip_info_init)
    i.drv_chip_rx_info_check                 0x000154f4   Section        0  drv_chip_info.o(i.drv_chip_rx_info_check)
    i.drv_chip_rx_init_done                  0x000155a4   Section        0  drv_chip_info.o(i.drv_chip_rx_init_done)
    i.drv_common_enable_systick              0x000155b8   Section        0  drv_common.o(i.drv_common_enable_systick)
    i.drv_common_system_init                 0x00015610   Section        0  drv_common.o(i.drv_common_system_init)
    i.drv_crgu_config_reset_modules          0x00015618   Section        0  drv_crgu.o(i.drv_crgu_config_reset_modules)
    i.drv_crgu_set_ahb_pre_div               0x00015628   Section        0  drv_crgu.o(i.drv_crgu_set_ahb_pre_div)
    i.drv_crgu_set_ahb_src                   0x0001563c   Section        0  drv_crgu.o(i.drv_crgu_set_ahb_src)
    i.drv_crgu_set_clock                     0x00015650   Section        0  drv_crgu.o(i.drv_crgu_set_clock)
    i.drv_crgu_set_dpi_mux_src               0x00015670   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_mux_src)
    i.drv_crgu_set_dpi_pre_div               0x00015684   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_pre_div)
    i.drv_crgu_set_dpi_pre_src               0x0001569c   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_pre_src)
    i.drv_crgu_set_dsc_core_div              0x000156b0   Section        0  drv_crgu.o(i.drv_crgu_set_dsc_core_div)
    i.drv_crgu_set_dsco_src                  0x000156c4   Section        0  drv_crgu.o(i.drv_crgu_set_dsco_src)
    i.drv_crgu_set_dsco_src_div              0x000156d8   Section        0  drv_crgu.o(i.drv_crgu_set_dsco_src_div)
    i.drv_crgu_set_fb_div                    0x000156ec   Section        0  drv_crgu.o(i.drv_crgu_set_fb_div)
    i.drv_crgu_set_fb_src                    0x00015700   Section        0  drv_crgu.o(i.drv_crgu_set_fb_src)
    i.drv_crgu_set_lcdc_div                  0x00015714   Section        0  drv_crgu.o(i.drv_crgu_set_lcdc_div)
    i.drv_crgu_set_lcdc_src                  0x00015728   Section        0  drv_crgu.o(i.drv_crgu_set_lcdc_src)
    i.drv_crgu_set_mipi_cfg_src              0x0001573c   Section        0  drv_crgu.o(i.drv_crgu_set_mipi_cfg_src)
    i.drv_crgu_set_mipi_ref_src              0x00015750   Section        0  drv_crgu.o(i.drv_crgu_set_mipi_ref_src)
    i.drv_crgu_set_reset                     0x00015768   Section        0  drv_crgu.o(i.drv_crgu_set_reset)
    i.drv_crgu_set_rxbr_div                  0x00015780   Section        0  drv_crgu.o(i.drv_crgu_set_rxbr_div)
    i.drv_crgu_set_rxbr_src                  0x00015794   Section        0  drv_crgu.o(i.drv_crgu_set_rxbr_src)
    i.drv_crgu_set_vidc_src                  0x000157a8   Section        0  drv_crgu.o(i.drv_crgu_set_vidc_src)
    i.drv_dma_clear_flag                     0x000157bc   Section        0  drv_dma.o(i.drv_dma_clear_flag)
    i.drv_dma_create_handle                  0x000157d4   Section        0  drv_dma.o(i.drv_dma_create_handle)
    i.drv_dma_disenable_channel              0x000157f0   Section        0  drv_dma.o(i.drv_dma_disenable_channel)
    i.drv_dma_enable_channel                 0x00015800   Section        0  drv_dma.o(i.drv_dma_enable_channel)
    i.drv_dma_enable_channel_interrupts      0x00015810   Section        0  drv_dma.o(i.drv_dma_enable_channel_interrupts)
    i.drv_dma_get_channel_flag               0x00015834   Section        0  drv_dma.o(i.drv_dma_get_channel_flag)
    i.drv_dma_irq_handler                    0x00015840   Section        0  drv_dma.o(i.drv_dma_irq_handler)
    i.drv_dma_prepar_transfer                0x000158d0   Section        0  drv_dma.o(i.drv_dma_prepar_transfer)
    i.drv_dma_set_burst                      0x000158e2   Section        0  drv_dma.o(i.drv_dma_set_burst)
    i.drv_dma_set_callback                   0x000158fc   Section        0  drv_dma.o(i.drv_dma_set_callback)
    i.drv_dma_set_transfer                   0x00015904   Section        0  drv_dma.o(i.drv_dma_set_transfer)
    i.drv_dsc_dec_convert_pps_rc_parameter   0x00015948   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter)
    i.drv_dsc_dec_disable                    0x0001597e   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    i.drv_dsc_dec_enable                     0x0001598c   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    i.drv_dsc_dec_get_nslc                   0x00015a00   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    i.drv_dsc_dec_set_u8_pps                 0x00015a0a   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps)
    i.drv_dsi_rx_calc_ipi_tx_delay           0x00015a34   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    i.drv_dsi_rx_enable_irq                  0x00015b38   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    i.drv_dsi_rx_get_color_bpp               0x00015b78   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    drv_dsi_rx_get_color_bpp                 0x00015b79   Thumb Code    62  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    i.drv_dsi_rx_get_color_pcc               0x00015bc8   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    drv_dsi_rx_get_color_pcc                 0x00015bc9   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    i.drv_dsi_rx_get_compression_en          0x00015be4   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    i.drv_dsi_rx_get_max_ret_size            0x00015bec   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size)
    i.drv_dsi_rx_power_up                    0x00015bf2   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    i.drv_dsi_rx_set_ctrl_cfg                0x00015c00   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    i.drv_dsi_rx_set_ddi_cfg                 0x00015c20   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    i.drv_dsi_rx_set_ipi_cfg                 0x00015c30   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    i.drv_dsi_rx_set_lane_swap               0x00015c40   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    i.drv_dsi_rx_set_resp_cnt                0x00015c86   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    i.drv_dsi_rx_set_up_phy                  0x00015cac   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    i.drv_dsi_rx_shut_down                   0x00015db0   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    i.drv_dsi_tx_command_header              0x00015dbe   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    i.drv_dsi_tx_command_mode_cfg            0x00015dd2   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    i.drv_dsi_tx_config_eotp                 0x00015e3e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    i.drv_dsi_tx_config_int                  0x00015e56   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    i.drv_dsi_tx_dpi_lpcmd_time              0x00015e5e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    i.drv_dsi_tx_dpi_mode                    0x00015e66   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    i.drv_dsi_tx_dpi_polarity                0x00015e70   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    i.drv_dsi_tx_edpi_cmd_size               0x00015e94   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    i.drv_dsi_tx_get_cmd_status              0x00015e98   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    i.drv_dsi_tx_mode                        0x00015e9c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    i.drv_dsi_tx_phy_clock_lane_auto_lp      0x00015ea0   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    i.drv_dsi_tx_phy_clock_lane_req_hs       0x00015eb8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    i.drv_dsi_tx_phy_lane_mode               0x00015ed2   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    i.drv_dsi_tx_phy_status_ready            0x00015ede   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    i.drv_dsi_tx_phy_status_stopstate        0x00015f42   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    i.drv_dsi_tx_phy_test_setup              0x00015f80   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    i.drv_dsi_tx_phy_time_cfg                0x000160b4   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    i.drv_dsi_tx_powerup                     0x000160d2   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    i.drv_dsi_tx_response_mode               0x000160da   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    i.drv_dsi_tx_set_bta_ack                 0x000160f6   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    i.drv_dsi_tx_set_esc_div                 0x0001610e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    i.drv_dsi_tx_set_int                     0x0001611c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    i.drv_dsi_tx_set_time_out_div            0x0001615c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    i.drv_dsi_tx_set_video_chunk             0x0001616c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    i.drv_dsi_tx_set_video_timing            0x00016174   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    i.drv_dsi_tx_shutdown                    0x00016196   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    i.drv_dsi_tx_timeout_cfg                 0x0001619e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    i.drv_dsi_tx_video_mode_cfg              0x000161c4   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    i.drv_dsi_tx_video_mode_disable_hact_cmd 0x0001626e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_disable_hact_cmd)
    i.drv_dsi_tx_video_mode_set_lp_cmd       0x00016284   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd)
    i.drv_efuse_enter_inactive               0x0001629c   Section        0  drv_efuse.o(i.drv_efuse_enter_inactive)
    i.drv_efuse_int_enable                   0x000162ca   Section        0  drv_efuse.o(i.drv_efuse_int_enable)
    i.drv_efuse_read                         0x000162d6   Section        0  drv_efuse.o(i.drv_efuse_read)
    i.drv_efuse_read_req                     0x00016308   Section        0  drv_efuse.o(i.drv_efuse_read_req)
    i.drv_gpio_get_input_data                0x00016320   Section        0  drv_gpio.o(i.drv_gpio_get_input_data)
    i.drv_gpio_register_ap_reset_callback    0x00016338   Section        0  drv_gpio.o(i.drv_gpio_register_ap_reset_callback)
    i.drv_gpio_register_callback             0x00016344   Section        0  drv_gpio.o(i.drv_gpio_register_callback)
    i.drv_gpio_set_int                       0x00016358   Section        0  drv_gpio.o(i.drv_gpio_set_int)
    i.drv_gpio_set_ioe                       0x000163a8   Section        0  drv_gpio.o(i.drv_gpio_set_ioe)
    i.drv_gpio_set_mode0                     0x000163c8   Section        0  drv_gpio.o(i.drv_gpio_set_mode0)
    i.drv_gpio_set_mode1                     0x000163d8   Section        0  drv_gpio.o(i.drv_gpio_set_mode1)
    i.drv_gpio_set_mode2                     0x000163e8   Section        0  drv_gpio.o(i.drv_gpio_set_mode2)
    i.drv_gpio_set_mode3                     0x000163f8   Section        0  drv_gpio.o(i.drv_gpio_set_mode3)
    i.drv_gpio_set_output_data               0x00016408   Section        0  hal_gpio.o(i.drv_gpio_set_output_data)
    drv_gpio_set_output_data                 0x00016409   Thumb Code    26  hal_gpio.o(i.drv_gpio_set_output_data)
    i.drv_gpio_set_pull_state                0x00016428   Section        0  drv_gpio.o(i.drv_gpio_set_pull_state)
    i.drv_i2c0_set_callback                  0x00016558   Section        0  drv_i2c_slave.o(i.drv_i2c0_set_callback)
    i.drv_i2c1_set_callback                  0x00016564   Section        0  drv_i2c_master.o(i.drv_i2c1_set_callback)
    i.drv_i2c_dma_callback                   0x00016570   Section        0  drv_i2c_dma.o(i.drv_i2c_dma_callback)
    drv_i2c_dma_callback                     0x00016571   Thumb Code    40  drv_i2c_dma.o(i.drv_i2c_dma_callback)
    i.drv_i2c_dma_init                       0x000165a4   Section        0  drv_i2c_dma.o(i.drv_i2c_dma_init)
    i.drv_i2c_enable_rx_dma                  0x00016650   Section        0  drv_i2c_dma.o(i.drv_i2c_enable_rx_dma)
    i.drv_i2c_enable_tx_dma                  0x0001666a   Section        0  drv_i2c_dma.o(i.drv_i2c_enable_tx_dma)
    i.drv_i2c_m_clear_it_pending_bit         0x00016684   Section        0  drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit)
    i.drv_i2c_m_enable                       0x000166e4   Section        0  drv_i2c_master.o(i.drv_i2c_m_enable)
    i.drv_i2c_m_enable_intr                  0x000166f4   Section        0  drv_i2c_master.o(i.drv_i2c_m_enable_intr)
    i.drv_i2c_master_init                    0x0001672c   Section        0  drv_i2c_master.o(i.drv_i2c_master_init)
    i.drv_i2c_master_read_dma                0x000167b8   Section        0  drv_i2c_dma.o(i.drv_i2c_master_read_dma)
    i.drv_i2c_master_write_dma               0x00016814   Section        0  drv_i2c_dma.o(i.drv_i2c_master_write_dma)
    i.drv_i2c_master_write_read_cmd          0x00016850   Section        0  drv_i2c_dma.o(i.drv_i2c_master_write_read_cmd)
    drv_i2c_master_write_read_cmd            0x00016851   Thumb Code    62  drv_i2c_dma.o(i.drv_i2c_master_write_read_cmd)
    i.drv_i2c_s_clear_it_pending_bit         0x0001688e   Section        0  drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit)
    i.drv_i2c_s_config_intr                  0x000168d0   Section        0  drv_i2c_slave.o(i.drv_i2c_s_config_intr)
    i.drv_i2c_s_enable                       0x000168d4   Section        0  drv_i2c_slave.o(i.drv_i2c_s_enable)
    i.drv_i2c_s_get_fifo_status              0x000168dc   Section        0  drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status)
    i.drv_i2c_s_set_intr                     0x000168f0   Section        0  drv_i2c_slave.o(i.drv_i2c_s_set_intr)
    i.drv_i2c_s_write_data                   0x00016940   Section        0  drv_i2c_slave.o(i.drv_i2c_s_write_data)
    i.drv_i2c_set_dma_irq_callback           0x0001695c   Section        0  drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback)
    i.drv_i2c_slave_init                     0x000169b4   Section        0  drv_i2c_slave.o(i.drv_i2c_slave_init)
    i.drv_i2c_slave_write_dma                0x000169e8   Section        0  drv_i2c_dma.o(i.drv_i2c_slave_write_dma)
    i.drv_lcdc_config_bypass                 0x00016a00   Section        0  drv_lcdc.o(i.drv_lcdc_config_bypass)
    i.drv_lcdc_config_ccm                    0x00016a18   Section        0  drv_lcdc.o(i.drv_lcdc_config_ccm)
    i.drv_lcdc_config_disp_mode              0x00016a48   Section        0  drv_lcdc.o(i.drv_lcdc_config_disp_mode)
    i.drv_lcdc_config_dpi_polarity           0x00016a5e   Section        0  drv_lcdc.o(i.drv_lcdc_config_dpi_polarity)
    i.drv_lcdc_config_dpi_timing             0x00016a82   Section        0  drv_lcdc.o(i.drv_lcdc_config_dpi_timing)
    i.drv_lcdc_config_edpi_mode              0x00016aa8   Section        0  drv_lcdc.o(i.drv_lcdc_config_edpi_mode)
    i.drv_lcdc_config_endianness             0x00016abe   Section        0  drv_lcdc.o(i.drv_lcdc_config_endianness)
    i.drv_lcdc_config_input_size             0x00016ad4   Section        0  drv_lcdc.o(i.drv_lcdc_config_input_size)
    i.drv_lcdc_config_int                    0x00016ae0   Section        0  drv_lcdc.o(i.drv_lcdc_config_int)
    i.drv_lcdc_config_int_single             0x00016afe   Section        0  drv_lcdc.o(i.drv_lcdc_config_int_single)
    i.drv_lcdc_config_overwrite              0x00016b20   Section        0  drv_lcdc.o(i.drv_lcdc_config_overwrite)
    i.drv_lcdc_config_overwrite_rgb          0x00016b42   Section        0  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    i.drv_lcdc_config_partial_display_area   0x00016b4e   Section        0  drv_lcdc.o(i.drv_lcdc_config_partial_display_area)
    i.drv_lcdc_config_partial_display_enable 0x00016b68   Section        0  drv_lcdc.o(i.drv_lcdc_config_partial_display_enable)
    i.drv_lcdc_config_scale_up_coef          0x00016b8a   Section        0  drv_lcdc.o(i.drv_lcdc_config_scale_up_coef)
    i.drv_lcdc_config_scale_up_step          0x00016ba4   Section        0  drv_lcdc.o(i.drv_lcdc_config_scale_up_step)
    i.drv_lcdc_config_src_parameter          0x00016bb0   Section        0  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    i.drv_lcdc_config_thresh                 0x00016bfc   Section        0  drv_lcdc.o(i.drv_lcdc_config_thresh)
    i.drv_lcdc_ctrl_flow                     0x00016c02   Section        0  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    i.drv_lcdc_enable_shadow_reg             0x00016c14   Section        0  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    i.drv_lcdc_set_int                       0x00016c34   Section        0  drv_lcdc.o(i.drv_lcdc_set_int)
    i.drv_lcdc_set_prefetch                  0x00016c74   Section        0  drv_lcdc.o(i.drv_lcdc_set_prefetch)
    i.drv_lcdc_set_video_hw_mode             0x00016c8c   Section        0  drv_lcdc.o(i.drv_lcdc_set_video_hw_mode)
    i.drv_lcdc_start                         0x00016ca0   Section        0  drv_lcdc.o(i.drv_lcdc_start)
    i.drv_memc_clear_status                  0x00016cc0   Section        0  drv_memc.o(i.drv_memc_clear_status)
    i.drv_memc_enable_irq                    0x00016ccc   Section        0  drv_memc.o(i.drv_memc_enable_irq)
    i.drv_memc_gen_a_tear_signal             0x00016d0c   Section        0  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    i.drv_memc_get_status                    0x00016d18   Section        0  drv_memc.o(i.drv_memc_get_status)
    i.drv_memc_rate_transfer_sel             0x00016d2a   Section        0  drv_memc.o(i.drv_memc_rate_transfer_sel)
    i.drv_memc_sel_vsync                     0x00016d3a   Section        0  drv_memc.o(i.drv_memc_sel_vsync)
    i.drv_memc_set_active_height             0x00016d48   Section        0  drv_memc.o(i.drv_memc_set_active_height)
    i.drv_memc_set_data_mode                 0x00016d5c   Section        0  drv_memc.o(i.drv_memc_set_data_mode)
    i.drv_memc_set_double_buffer             0x00016d68   Section        0  drv_memc.o(i.drv_memc_set_double_buffer)
    i.drv_memc_set_double_buffer_reverse     0x00016d78   Section        0  drv_memc.o(i.drv_memc_set_double_buffer_reverse)
    i.drv_memc_set_fs_en_conditions          0x00016d8a   Section        0  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    i.drv_memc_set_inten                     0x00016d9a   Section        0  drv_memc.o(i.drv_memc_set_inten)
    i.drv_memc_set_lcdc_st_conditions        0x00016db0   Section        0  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    i.drv_memc_set_ltpo_mode                 0x00016dc8   Section        0  drv_memc.o(i.drv_memc_set_ltpo_mode)
    i.drv_memc_set_tear_mode                 0x00016de2   Section        0  drv_memc.o(i.drv_memc_set_tear_mode)
    i.drv_memc_set_tear_waveform             0x00016df0   Section        0  drv_memc.o(i.drv_memc_set_tear_waveform)
    i.drv_memc_set_vidc_sync_cnt             0x00016e18   Section        0  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    i.drv_param_init_get_ccm                 0x00016e28   Section        0  drv_param_init.o(i.drv_param_init_get_ccm)
    i.drv_param_init_get_scld_filter_h       0x00016e30   Section        0  drv_param_init.o(i.drv_param_init_get_scld_filter_h)
    i.drv_param_init_get_scld_filter_v       0x00016e44   Section        0  drv_param_init.o(i.drv_param_init_get_scld_filter_v)
    i.drv_param_init_get_sclu_filter         0x00016e58   Section        0  drv_param_init.o(i.drv_param_init_get_sclu_filter)
    i.drv_param_init_set_ccm                 0x00016e60   Section        0  drv_param_init.o(i.drv_param_init_set_ccm)
    i.drv_param_p2r_filter_init              0x00016e74   Section        0  drv_param_init.o(i.drv_param_p2r_filter_init)
    i.drv_phy_enable_calibration             0x00016e98   Section        0  drv_phy_common.o(i.drv_phy_enable_calibration)
    i.drv_phy_get_calibration                0x00016ea8   Section        0  drv_phy_common.o(i.drv_phy_get_calibration)
    i.drv_phy_get_pll_para                   0x00016ee4   Section        0  drv_phy_common.o(i.drv_phy_get_pll_para)
    i.drv_phy_get_rate_para                  0x00016f44   Section        0  drv_phy_common.o(i.drv_phy_get_rate_para)
    i.drv_phy_test_clear                     0x00016f98   Section        0  drv_phy_common.o(i.drv_phy_test_clear)
    i.drv_phy_test_lock                      0x00016fa8   Section        0  drv_phy_common.o(i.drv_phy_test_lock)
    i.drv_phy_test_write_1_byte              0x00016fc0   Section        0  drv_phy_common.o(i.drv_phy_test_write_1_byte)
    i.drv_phy_test_write_2_byte              0x00016fe0   Section        0  drv_phy_common.o(i.drv_phy_test_write_2_byte)
    i.drv_phy_test_write_code                0x00017006   Section        0  drv_phy_common.o(i.drv_phy_test_write_code)
    i.drv_phy_test_write_data                0x00017024   Section        0  drv_phy_common.o(i.drv_phy_test_write_data)
    drv_phy_test_write_data                  0x00017025   Thumb Code    32  drv_phy_common.o(i.drv_phy_test_write_data)
    i.drv_pwr_set_cp_mode                    0x00017044   Section        0  drv_pwr.o(i.drv_pwr_set_cp_mode)
    i.drv_pwr_set_pvd_mode                   0x00017064   Section        0  drv_pwr.o(i.drv_pwr_set_pvd_mode)
    i.drv_pwr_set_system_clk_src             0x0001707c   Section        0  drv_pwr.o(i.drv_pwr_set_system_clk_src)
    i.drv_rx_phy_test_clear                  0x000170b4   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_clear)
    drv_rx_phy_test_clear                    0x000170b5   Thumb Code    12  drv_dsi_rx.o(i.drv_rx_phy_test_clear)
    i.drv_rx_phy_test_lock                   0x000170c0   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_lock)
    drv_rx_phy_test_lock                     0x000170c1   Thumb Code    16  drv_dsi_rx.o(i.drv_rx_phy_test_lock)
    i.drv_rx_phy_test_write_1_byte           0x000170d0   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte)
    drv_rx_phy_test_write_1_byte             0x000170d1   Thumb Code    20  drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte)
    i.drv_rx_phy_test_write_2_byte           0x000170e4   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte)
    drv_rx_phy_test_write_2_byte             0x000170e5   Thumb Code    22  drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte)
    i.drv_rxbr_clear_pkt_buffer              0x000170fa   Section        0  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    i.drv_rxbr_clear_status0                 0x00017104   Section        0  drv_rxbr.o(i.drv_rxbr_clear_status0)
    i.drv_rxbr_enable_irq                    0x00017108   Section        0  drv_rxbr.o(i.drv_rxbr_enable_irq)
    i.drv_rxbr_frame_drop_cfg                0x00017164   Section        0  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    i.drv_rxbr_get_clk                       0x00017178   Section        0  drv_rxbr.o(i.drv_rxbr_get_clk)
    i.drv_rxbr_get_col_addr                  0x000171dc   Section        0  drv_rxbr.o(i.drv_rxbr_get_col_addr)
    i.drv_rxbr_get_int_source                0x000171e0   Section        0  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    drv_rxbr_get_int_source                  0x000171e1   Thumb Code    18  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    i.drv_rxbr_get_page_addr                 0x000171f2   Section        0  drv_rxbr.o(i.drv_rxbr_get_page_addr)
    i.drv_rxbr_get_status0                   0x000171f6   Section        0  hal_internal_vsync.o(i.drv_rxbr_get_status0)
    drv_rxbr_get_status0                     0x000171f7   Thumb Code    18  hal_internal_vsync.o(i.drv_rxbr_get_status0)
    i.drv_rxbr_hline_rcv0_cfg                0x00017208   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg)
    i.drv_rxbr_hline_rcv_cfg                 0x00017214   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    i.drv_rxbr_register_irq0_callback        0x0001721c   Section        0  drv_rxbr.o(i.drv_rxbr_register_irq0_callback)
    i.drv_rxbr_register_irq1_callback        0x00017228   Section        0  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    i.drv_rxbr_set_ack_pkt_header            0x00017234   Section        0  drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header)
    i.drv_rxbr_set_cmd_filter                0x00017248   Section        0  drv_rxbr.o(i.drv_rxbr_set_cmd_filter)
    i.drv_rxbr_set_color_format              0x00017314   Section        0  drv_rxbr.o(i.drv_rxbr_set_color_format)
    i.drv_rxbr_set_inten                     0x00017328   Section        0  drv_rxbr.o(i.drv_rxbr_set_inten)
    i.drv_rxbr_set_ltpo_drop_th              0x0001733c   Section        0  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    i.drv_rxbr_set_usr_cfg                   0x0001734c   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    i.drv_rxbr_set_usr_col                   0x00017372   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    i.drv_rxbr_set_usr_row                   0x0001737a   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    i.drv_spi_m_read_data                    0x00017384   Section        0  drv_spi_master.o(i.drv_spi_m_read_data)
    i.drv_swire_set_int                      0x000173a4   Section        0  drv_swire.o(i.drv_swire_set_int)
    i.drv_swire_set_power_down               0x000173f8   Section        0  drv_swire.o(i.drv_swire_set_power_down)
    i.drv_sys_cfg_clear_all_int              0x00017414   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    i.drv_sys_cfg_clear_pending              0x00017420   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    i.drv_sys_cfg_sel_ap_rst_lvl_trig        0x00017448   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig)
    i.drv_sys_cfg_sel_ap_rst_trig            0x00017460   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig)
    i.drv_sys_cfg_sel_gpio_group             0x0001747c   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group)
    i.drv_sys_cfg_sel_int_trig               0x000174a0   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig)
    i.drv_sys_cfg_set_dma_rx_req             0x000174c4   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req)
    i.drv_sys_cfg_set_dma_tx_req             0x000174d4   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req)
    i.drv_sys_cfg_set_int                    0x000174e4   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    i.drv_timer_clear_status_flags           0x00017508   Section        0  drv_timer.o(i.drv_timer_clear_status_flags)
    drv_timer_clear_status_flags             0x00017509   Thumb Code    26  drv_timer.o(i.drv_timer_clear_status_flags)
    i.drv_timer_enable                       0x00017522   Section        0  drv_timer.o(i.drv_timer_enable)
    i.drv_timer_get_instance                 0x00017544   Section        0  drv_timer.o(i.drv_timer_get_instance)
    i.drv_timer_get_prescaler                0x00017554   Section        0  drv_timer.o(i.drv_timer_get_prescaler)
    i.drv_timer_handle_interrupt             0x00017564   Section        0  drv_timer.o(i.drv_timer_handle_interrupt)
    drv_timer_handle_interrupt               0x00017565   Thumb Code    62  drv_timer.o(i.drv_timer_handle_interrupt)
    i.drv_timer_register_callback            0x000175a8   Section        0  drv_timer.o(i.drv_timer_register_callback)
    i.drv_timer_set_compare_val              0x000175bc   Section        0  drv_timer.o(i.drv_timer_set_compare_val)
    i.drv_timer_set_int                      0x000175cc   Section        0  drv_timer.o(i.drv_timer_set_int)
    i.drv_timer_set_prescaler                0x00017620   Section        0  drv_timer.o(i.drv_timer_set_prescaler)
    i.drv_tx_phy_test_clear                  0x00017648   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_clear)
    drv_tx_phy_test_clear                    0x00017649   Thumb Code    10  drv_dsi_tx.o(i.drv_tx_phy_test_clear)
    i.drv_tx_phy_test_enter                  0x00017652   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    i.drv_tx_phy_test_exit                   0x0001766e   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    i.drv_tx_phy_test_write_1_byte           0x0001768a   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte)
    drv_tx_phy_test_write_1_byte             0x0001768b   Thumb Code    18  drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte)
    i.drv_tx_phy_test_write_2_byte           0x0001769c   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte)
    drv_tx_phy_test_write_2_byte             0x0001769d   Thumb Code    20  drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte)
    i.drv_tx_phy_test_write_code             0x000176b0   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    drv_tx_phy_test_write_code               0x000176b1   Thumb Code    16  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    i.drv_vidc_clear_irq                     0x000176c0   Section        0  drv_vidc.o(i.drv_vidc_clear_irq)
    i.drv_vidc_enable                        0x000176c8   Section        0  drv_vidc.o(i.drv_vidc_enable)
    i.drv_vidc_enable_irq                    0x000176e0   Section        0  drv_vidc.o(i.drv_vidc_enable_irq)
    i.drv_vidc_get_irq_status                0x00017720   Section        0  drv_vidc.o(i.drv_vidc_get_irq_status)
    i.drv_vidc_init_module_enable            0x00017734   Section        0  drv_vidc.o(i.drv_vidc_init_module_enable)
    i.drv_vidc_register_callback             0x0001775c   Section        0  drv_vidc.o(i.drv_vidc_register_callback)
    i.drv_vidc_reset                         0x00017768   Section        0  drv_vidc.o(i.drv_vidc_reset)
    i.drv_vidc_set_dst_parameter             0x0001776e   Section        0  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    i.drv_vidc_set_irqen                     0x000177aa   Section        0  drv_vidc.o(i.drv_vidc_set_irqen)
    i.drv_vidc_set_mirror                    0x000177be   Section        0  drv_vidc.o(i.drv_vidc_set_mirror)
    i.drv_vidc_set_p2r_hcoef0                0x000177ce   Section        0  drv_vidc.o(i.drv_vidc_set_p2r_hcoef0)
    i.drv_vidc_set_p2r_hinitb                0x000177d6   Section        0  drv_vidc.o(i.drv_vidc_set_p2r_hinitb)
    i.drv_vidc_set_p2r_hinitr                0x000177fc   Section        0  drv_vidc.o(i.drv_vidc_set_p2r_hinitr)
    i.drv_vidc_set_pentile_swap              0x00017824   Section        0  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    i.drv_vidc_set_pu_ctrl                   0x0001783c   Section        0  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    i.drv_vidc_set_rotation                  0x00017846   Section        0  drv_vidc.o(i.drv_vidc_set_rotation)
    i.drv_vidc_set_scld_hcoef0               0x00017856   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    i.drv_vidc_set_scld_hcoef1               0x00017860   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    i.drv_vidc_set_scld_step                 0x0001786a   Section        0  drv_vidc.o(i.drv_vidc_set_scld_step)
    i.drv_vidc_set_scld_vcoef0               0x0001787c   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    i.drv_vidc_set_scld_vcoef1               0x00017886   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    i.drv_vidc_set_src_parameter             0x00017890   Section        0  drv_vidc.o(i.drv_vidc_set_src_parameter)
    i.drv_wdg_clear_counter                  0x000178a8   Section        0  drv_wdg.o(i.drv_wdg_clear_counter)
    i.drv_wdg_clear_edge_flag                0x000178b8   Section        0  drv_wdg.o(i.drv_wdg_clear_edge_flag)
    drv_wdg_clear_edge_flag                  0x000178b9   Thumb Code    12  drv_wdg.o(i.drv_wdg_clear_edge_flag)
    i.drv_wdg_read_edge_flag                 0x000178c8   Section        0  drv_wdg.o(i.drv_wdg_read_edge_flag)
    drv_wdg_read_edge_flag                   0x000178c9   Thumb Code    10  drv_wdg.o(i.drv_wdg_read_edge_flag)
    i.drv_wdg_set_int                        0x000178d8   Section        0  drv_wdg.o(i.drv_wdg_set_int)
    i.fls_clr_interrupt_flag                 0x00017918   Section        0  drv_fls.o(i.fls_clr_interrupt_flag)
    i.fputc                                  0x00017922   Section        0  tau_log.o(i.fputc)
    i.hal_dsi_rx_ctrl_create_handle          0x00017938   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    i.hal_dsi_rx_ctrl_deinit                 0x0001796c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit)
    i.hal_dsi_rx_ctrl_dsc_async_handler      0x00017a08   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler)
    i.hal_dsi_rx_ctrl_gen_a_tear_signal      0x00017a8c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal)
    i.hal_dsi_rx_ctrl_get_max_ret_size       0x00017ab4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size)
    i.hal_dsi_rx_ctrl_hight_performan_mode   0x00017adc   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode)
    i.hal_dsi_rx_ctrl_init                   0x00017b40   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    i.hal_dsi_rx_ctrl_init_clk               0x00017bd8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    hal_dsi_rx_ctrl_init_clk                 0x00017bd9   Thumb Code   332  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    i.hal_dsi_rx_ctrl_init_dsi_rx            0x00017d7c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    hal_dsi_rx_ctrl_init_dsi_rx              0x00017d7d   Thumb Code   184  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    i.hal_dsi_rx_ctrl_init_memc              0x00017e54   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    hal_dsi_rx_ctrl_init_memc                0x00017e55   Thumb Code   334  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    i.hal_dsi_rx_ctrl_init_rxbr              0x00017fac   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    hal_dsi_rx_ctrl_init_rxbr                0x00017fad   Thumb Code   312  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    i.hal_dsi_rx_ctrl_init_vidc              0x000180f4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    hal_dsi_rx_ctrl_init_vidc                0x000180f5   Thumb Code   544  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    i.hal_dsi_rx_ctrl_pre_init_pps           0x00018320   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    i.hal_dsi_rx_ctrl_send_ack_cmd           0x0001835c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd)
    i.hal_dsi_rx_ctrl_set_cus_sync_line      0x0001844c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line)
    i.hal_dsi_rx_ctrl_set_hw_tear_mode       0x00018480   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode)
    i.hal_dsi_rx_ctrl_set_ipi_cfg            0x000184b4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    hal_dsi_rx_ctrl_set_ipi_cfg              0x000184b5   Thumb Code    50  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    i.hal_dsi_rx_ctrl_set_rxbr_clk           0x000184ec   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk)
    hal_dsi_rx_ctrl_set_rxbr_clk             0x000184ed   Thumb Code   114  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk)
    i.hal_dsi_rx_ctrl_set_sw_tear_mode       0x00018560   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode)
    i.hal_dsi_rx_ctrl_set_tear_mode_ex       0x00018594   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex)
    i.hal_dsi_rx_ctrl_start                  0x000185a4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    i.hal_dsi_rx_ctrl_stop                   0x000185e0   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop)
    i.hal_dsi_rx_ctrl_toggle_resolution      0x0001861c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    i.hal_dsi_tx_calc_video_chunks           0x0001863c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks)
    hal_dsi_tx_calc_video_chunks             0x0001863d   Thumb Code   384  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks)
    i.hal_dsi_tx_config_params_for_lane_rate 0x000187cc   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate)
    hal_dsi_tx_config_params_for_lane_rate   0x000187cd   Thumb Code    42  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate)
    i.hal_dsi_tx_count_lane_rate             0x00018800   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate)
    hal_dsi_tx_count_lane_rate               0x00018801   Thumb Code  1022  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate)
    i.hal_dsi_tx_ctrl_create_handle          0x00018c50   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    i.hal_dsi_tx_ctrl_deinit                 0x00018c7c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit)
    i.hal_dsi_tx_ctrl_enter_init_panel_mode  0x00018d00   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode)
    i.hal_dsi_tx_ctrl_exit_init_panel_mode   0x00018d4c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode)
    i.hal_dsi_tx_ctrl_init                   0x00018d74   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    i.hal_dsi_tx_ctrl_init_clk               0x00018e18   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    hal_dsi_tx_ctrl_init_clk                 0x00018e19   Thumb Code    36  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    i.hal_dsi_tx_ctrl_panel_reset_pin        0x00018e3c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin)
    i.hal_dsi_tx_ctrl_set_ccm                0x00018e48   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm)
    i.hal_dsi_tx_ctrl_set_overwrite_rgb      0x00018e68   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    i.hal_dsi_tx_ctrl_set_partial_disp       0x00018e7c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp)
    i.hal_dsi_tx_ctrl_set_partial_disp_area  0x00018e8c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area)
    i.hal_dsi_tx_ctrl_start                  0x00018eb0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    i.hal_dsi_tx_ctrl_stop                   0x00018f4c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop)
    i.hal_dsi_tx_ctrl_write_array_cmd        0x00018f90   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd)
    i.hal_dsi_tx_ctrl_write_cmd              0x00019068   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    i.hal_dsi_tx_init_data_mode              0x00019118   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode)
    hal_dsi_tx_init_data_mode                0x00019119   Thumb Code    58  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode)
    i.hal_dsi_tx_init_dpi_cfg                0x0001915c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg)
    hal_dsi_tx_init_dpi_cfg                  0x0001915d   Thumb Code    42  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg)
    i.hal_dsi_tx_init_interrupt              0x0001918c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt)
    hal_dsi_tx_init_interrupt                0x0001918d   Thumb Code    28  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt)
    i.hal_dsi_tx_init_phy_cfg                0x000191ac   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    hal_dsi_tx_init_phy_cfg                  0x000191ad   Thumb Code    28  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    i.hal_dsi_tx_init_remains                0x000191cc   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains)
    hal_dsi_tx_init_remains                  0x000191cd   Thumb Code   142  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains)
    i.hal_dsi_tx_init_video_mode             0x00019260   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode)
    hal_dsi_tx_init_video_mode               0x00019261   Thumb Code    82  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode)
    i.hal_dsi_tx_send_cmd                    0x000192b8   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    hal_dsi_tx_send_cmd                      0x000192b9   Thumb Code    60  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    i.hal_gpio_ctrl_eint                     0x000192fc   Section        0  hal_gpio.o(i.hal_gpio_ctrl_eint)
    i.hal_gpio_get_input_data                0x00019314   Section        0  hal_gpio.o(i.hal_gpio_get_input_data)
    i.hal_gpio_init_eint                     0x00019328   Section        0  hal_gpio.o(i.hal_gpio_init_eint)
    i.hal_gpio_init_input                    0x00019368   Section        0  hal_gpio.o(i.hal_gpio_init_input)
    i.hal_gpio_init_output                   0x00019388   Section        0  hal_gpio.o(i.hal_gpio_init_output)
    i.hal_gpio_reg_eint_cb                   0x000193b0   Section        0  hal_gpio.o(i.hal_gpio_reg_eint_cb)
    i.hal_gpio_set_ap_reset_int              0x000193c8   Section        0  hal_gpio.o(i.hal_gpio_set_ap_reset_int)
    i.hal_gpio_set_mode                      0x00019418   Section        0  hal_gpio.o(i.hal_gpio_set_mode)
    i.hal_gpio_set_output_data               0x00019478   Section        0  hal_gpio.o(i.hal_gpio_set_output_data)
    i.hal_gpio_set_pull_state                0x00019480   Section        0  hal_gpio.o(i.hal_gpio_set_pull_state)
    i.hal_i2c_m_dma_init                     0x000194a0   Section        0  hal_i2c_master.o(i.hal_i2c_m_dma_init)
    i.hal_i2c_m_dma_read                     0x0001950c   Section        0  hal_i2c_master.o(i.hal_i2c_m_dma_read)
    i.hal_i2c_m_dma_write                    0x0001952c   Section        0  hal_i2c_master.o(i.hal_i2c_m_dma_write)
    i.hal_i2c_m_transfer_complate            0x00019548   Section        0  hal_i2c_master.o(i.hal_i2c_m_transfer_complate)
    i.hal_i2c_master_irq_callback            0x00019554   Section        0  hal_i2c_master.o(i.hal_i2c_master_irq_callback)
    hal_i2c_master_irq_callback              0x00019555   Thumb Code    24  hal_i2c_master.o(i.hal_i2c_master_irq_callback)
    i.hal_i2c_s_dma_user_callback            0x00019574   Section        0  hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback)
    hal_i2c_s_dma_user_callback              0x00019575   Thumb Code    12  hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback)
    i.hal_i2c_s_dma_write                    0x00019584   Section        0  hal_i2c_slave.o(i.hal_i2c_s_dma_write)
    i.hal_i2c_s_init                         0x000195d0   Section        0  hal_i2c_slave.o(i.hal_i2c_s_init)
    i.hal_i2c_s_nonblocking_read             0x00019698   Section        0  hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read)
    i.hal_i2c_s_set_transfer                 0x000196ac   Section        0  hal_i2c_slave.o(i.hal_i2c_s_set_transfer)
    i.hal_i2c_slave_irq_callback             0x000196b8   Section        0  hal_i2c_slave.o(i.hal_i2c_slave_irq_callback)
    hal_i2c_slave_irq_callback               0x000196b9   Thumb Code   356  hal_i2c_slave.o(i.hal_i2c_slave_irq_callback)
    i.hal_internal_init_memc                 0x0001982c   Section        0  hal_internal_vsync.o(i.hal_internal_init_memc)
    i.hal_internal_sync_get_fb_setting       0x00019928   Section        0  hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting)
    i.hal_internal_sync_get_hight_performan_mode 0x00019938   Section        0  hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode)
    i.hal_internal_sync_input_resolution_change 0x00019948   Section        0  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    i.hal_internal_update_dpi_param          0x00019b74   Section        0  hal_internal_vsync.o(i.hal_internal_update_dpi_param)
    i.hal_internal_video_mode_auto_sync      0x00019b84   Section        0  hal_internal_vsync.o(i.hal_internal_video_mode_auto_sync)
    i.hal_internal_vsync_deinit              0x00019cb0   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    i.hal_internal_vsync_get_rx_state        0x00019cd8   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state)
    i.hal_internal_vsync_get_sync_line       0x00019ce4   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    i.hal_internal_vsync_get_tear_mode       0x00019cfc   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_tear_mode)
    i.hal_internal_vsync_get_tx_state        0x00019d08   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    i.hal_internal_vsync_init_rx             0x00019d14   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    i.hal_internal_vsync_init_tx             0x00019e2c   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    i.hal_internal_vsync_set_auto_hw_filter  0x00019edc   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter)
    i.hal_internal_vsync_set_rx_state        0x00019ff8   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    i.hal_internal_vsync_set_sync_line       0x0001a00c   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line)
    i.hal_internal_vsync_set_tear_mode       0x0001a030   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    i.hal_internal_vsync_set_tx_state        0x0001a080   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    i.hal_lcdc_config_ccm                    0x0001a100   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm)
    hal_lcdc_config_ccm                      0x0001a101   Thumb Code    30  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm)
    i.hal_lcdc_config_remains                0x0001a124   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains)
    hal_lcdc_config_remains                  0x0001a125   Thumb Code    84  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains)
    i.hal_lcdc_config_rgb_to_pentile         0x0001a17c   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile)
    hal_lcdc_config_rgb_to_pentile           0x0001a17d   Thumb Code    14  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile)
    i.hal_lcdc_config_upscaler               0x0001a190   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler)
    hal_lcdc_config_upscaler                 0x0001a191   Thumb Code   348  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler)
    i.hal_lcdc_init_cfg                      0x0001a2f4   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    hal_lcdc_init_cfg                        0x0001a2f5   Thumb Code    78  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    i.hal_lcdc_init_clk                      0x0001a348   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    hal_lcdc_init_clk                        0x0001a349   Thumb Code   422  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    i.hal_lcdc_init_interrupt                0x0001a4f8   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt)
    hal_lcdc_init_interrupt                  0x0001a4f9   Thumb Code    58  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt)
    i.hal_spi_m_clear_rxfifo                 0x0001a538   Section        0  hal_spi_master.o(i.hal_spi_m_clear_rxfifo)
    i.hal_swire_open                         0x0001a546   Section        0  hal_swire.o(i.hal_swire_open)
    i.hal_system_enable_systick              0x0001a55c   Section        0  hal_system.o(i.hal_system_enable_systick)
    i.hal_system_init                        0x0001a564   Section        0  hal_system.o(i.hal_system_init)
    i.hal_system_init_console                0x0001a5ec   Section        0  hal_system.o(i.hal_system_init_console)
    i.hal_system_set_phy_calibration         0x0001a608   Section        0  hal_system.o(i.hal_system_set_phy_calibration)
    i.hal_system_set_pvd                     0x0001a610   Section        0  hal_system.o(i.hal_system_set_pvd)
    i.hal_system_set_vcc                     0x0001a618   Section        0  hal_system.o(i.hal_system_set_vcc)
    i.hal_timer_init                         0x0001a620   Section        0  hal_timer.o(i.hal_timer_init)
    i.hal_timer_start                        0x0001a63c   Section        0  hal_timer.o(i.hal_timer_start)
    i.hal_timer_stop                         0x0001a684   Section        0  hal_timer.o(i.hal_timer_stop)
    i.hal_uart_init                          0x0001a6ac   Section        0  hal_uart.o(i.hal_uart_init)
    i.hal_uart_transmit_blocking             0x0001a738   Section        0  hal_uart.o(i.hal_uart_transmit_blocking)
    i.handle_init                            0x0001a748   Section        0  irq_redirect .o(i.handle_init)
    i.init_mipi_tx                           0x0001a858   Section        0  ap_demo.o(i.init_mipi_tx)
    init_mipi_tx                             0x0001a859   Thumb Code    96  ap_demo.o(i.init_mipi_tx)
    i.init_panel                             0x0001a8bc   Section        0  ap_demo.o(i.init_panel)
    init_panel                               0x0001a8bd   Thumb Code   126  ap_demo.o(i.init_panel)
    i.main                                   0x0001a944   Section        0  main.o(i.main)
    i.open_mipi_rx                           0x0001a950   Section        0  ap_demo.o(i.open_mipi_rx)
    open_mipi_rx                             0x0001a951   Thumb Code   138  ap_demo.o(i.open_mipi_rx)
    i.pps_update_handle                      0x0001a9f0   Section        0  ap_demo.o(i.pps_update_handle)
    pps_update_handle                        0x0001a9f1   Thumb Code    80  ap_demo.o(i.pps_update_handle)
    i.rx_get_dcs_packet_data                 0x0001aa44   Section        0  hal_internal_vsync.o(i.rx_get_dcs_packet_data)
    rx_get_dcs_packet_data                   0x0001aa45   Thumb Code   654  hal_internal_vsync.o(i.rx_get_dcs_packet_data)
    i.rx_partial_update                      0x0001ae38   Section        0  hal_internal_vsync.o(i.rx_partial_update)
    rx_partial_update                        0x0001ae39   Thumb Code   358  hal_internal_vsync.o(i.rx_partial_update)
    i.rx_receive_packet                      0x0001afb0   Section        0  hal_internal_vsync.o(i.rx_receive_packet)
    rx_receive_packet                        0x0001afb1   Thumb Code   128  hal_internal_vsync.o(i.rx_receive_packet)
    i.rx_receive_pps                         0x0001b03c   Section        0  hal_internal_vsync.o(i.rx_receive_pps)
    rx_receive_pps                           0x0001b03d   Thumb Code   268  hal_internal_vsync.o(i.rx_receive_pps)
    i.rxbr_irq0_callback                     0x0001b1bc   Section        0  hal_internal_vsync.o(i.rxbr_irq0_callback)
    rxbr_irq0_callback                       0x0001b1bd   Thumb Code   158  hal_internal_vsync.o(i.rxbr_irq0_callback)
    i.rxbr_irq1_callback                     0x0001b260   Section        0  hal_internal_vsync.o(i.rxbr_irq1_callback)
    rxbr_irq1_callback                       0x0001b261   Thumb Code   324  hal_internal_vsync.o(i.rxbr_irq1_callback)
    i.soft_gen_te                            0x0001b43c   Section        0  hal_internal_vsync.o(i.soft_gen_te)
    soft_gen_te                              0x0001b43d   Thumb Code   166  hal_internal_vsync.o(i.soft_gen_te)
    i.soft_gen_te_double_buffer              0x0001b500   Section        0  hal_internal_vsync.o(i.soft_gen_te_double_buffer)
    soft_gen_te_double_buffer                0x0001b501   Thumb Code   166  hal_internal_vsync.o(i.soft_gen_te_double_buffer)
    i.soft_timer3_cb                         0x0001b5c0   Section        0  ap_demo.o(i.soft_timer3_cb)
    soft_timer3_cb                           0x0001b5c1   Thumb Code    36  ap_demo.o(i.soft_timer3_cb)
    i.sqrt                                   0x0001b5f0   Section        0  sqrt.o(i.sqrt)
    i.tp_heartbeat_exec                      0x0001b638   Section        0  ap_demo.o(i.tp_heartbeat_exec)
    i.vidc_callback                          0x0001b678   Section        0  hal_internal_vsync.o(i.vidc_callback)
    vidc_callback                            0x0001b679   Thumb Code   232  hal_internal_vsync.o(i.vidc_callback)
    i.vpre_err_reset                         0x0001b780   Section        0  hal_internal_vsync.o(i.vpre_err_reset)
    vpre_err_reset                           0x0001b781   Thumb Code   184  hal_internal_vsync.o(i.vpre_err_reset)
    i.vsync_set_te_mode                      0x0001b850   Section        0  hal_internal_vsync.o(i.vsync_set_te_mode)
    vsync_set_te_mode                        0x0001b851   Thumb Code   300  hal_internal_vsync.o(i.vsync_set_te_mode)
    .constdata                               0x0001ba1c   Section      248  ap_demo.o(.constdata)
    g_cus_rx_dcs_execute_table               0x0001ba1c   Data         120  ap_demo.o(.constdata)
    .constdata                               0x0001bb14   Section       36  hal_dsi_tx_ctrl.o(.constdata)
    .constdata                               0x0001bb38   Section      210  hal_gpio.o(.constdata)
    s_gpio_map                               0x0001bb38   Data         120  hal_gpio.o(.constdata)
    s_gpio_perf                              0x0001bbb0   Data          90  hal_gpio.o(.constdata)
    .constdata                               0x0001bc0c   Section       32  hal_i2c_slave.o(.constdata)
    sg_i2c_s_config                          0x0001bc0c   Data          32  hal_i2c_slave.o(.constdata)
    .constdata                               0x0001bc2c   Section     8528  app_tp_for_custom_s8.o(.constdata)
    .constdata                               0x0001dd7c   Section        1  app_tp_for_custom_s8.o(.constdata)
    .constdata                               0x0001dd80   Section        8  drv_param_init.o(.constdata)
    .constdata                               0x0001dd88   Section      390  drv_phy_common.o(.constdata)
    phy_para_mapping_h                       0x0001dd88   Data         184  drv_phy_common.o(.constdata)
    phy_para_mapping_l                       0x0001de40   Data         128  drv_phy_common.o(.constdata)
    phy_data_high_map                        0x0001dec0   Data          48  drv_phy_common.o(.constdata)
    phy_data_lp_map                          0x0001def0   Data          30  drv_phy_common.o(.constdata)
    .conststring                             0x0001df10   Section       72  hal_dsi_rx_ctrl.o(.conststring)
    .conststring                             0x0001df58   Section       67  hal_dsi_tx_ctrl.o(.conststring)
    .conststring                             0x0001df9c   Section      308  hal_internal_vsync.o(.conststring)
    .ARM.__AT_0x00070100                     0x00070100   Section      192  irq_redirect .o(.ARM.__AT_0x00070100)
    .data                                    0x000701d0   Section     7526  ap_demo.o(.data)
    start_display_on                         0x000701d0   Data           1  ap_demo.o(.data)
    g_need_enter_sleep_mode                  0x000701d1   Data           1  ap_demo.o(.data)
    g_mipi_path_off                          0x000701d2   Data           1  ap_demo.o(.data)
    phone_off_flag                           0x000701d3   Data           1  ap_demo.o(.data)
    g_exit_sleep_mode                        0x000701d4   Data           1  ap_demo.o(.data)
    panel_display_done                       0x000701d5   Data           1  ap_demo.o(.data)
    phone_power_on                           0x000701d6   Data           1  ap_demo.o(.data)
    g_calibration_flag                       0x000701db   Data           1  ap_demo.o(.data)
    bl_adj_flag                              0x000701df   Data           1  ap_demo.o(.data)
    b3_read_flag                             0x000701e1   Data           1  ap_demo.o(.data)
    c8_read_flag                             0x000701e2   Data           1  ap_demo.o(.data)
    c9_read_flag                             0x000701e3   Data           1  ap_demo.o(.data)
    c9_read_flag2                            0x000701e4   Data           1  ap_demo.o(.data)
    c9_read_flag3                            0x000701e5   Data           1  ap_demo.o(.data)
    flag_5a                                  0x000701e6   Data           1  ap_demo.o(.data)
    frame_rate                               0x000701e7   Data           1  ap_demo.o(.data)
    g_rx_ctrl_handle                         0x000701f8   Data           4  ap_demo.o(.data)
    g_tx_ctrl_handle                         0x000701fc   Data           4  ap_demo.o(.data)
    value_reg_df                             0x00070208   Data           4  ap_demo.o(.data)
    .data                                    0x00071f36   Section       23  app_tp_transfer.o(.data)
    s_spim_write                             0x00071f36   Data           1  app_tp_transfer.o(.data)
    s_screen_int_flag                        0x00071f37   Data           1  app_tp_transfer.o(.data)
    s_phone_reset_flag                       0x00071f38   Data           1  app_tp_transfer.o(.data)
    s_screen_int_transfer_status             0x00071f39   Data           1  app_tp_transfer.o(.data)
    s_screen_const_transfer_count            0x00071f3b   Data           1  app_tp_transfer.o(.data)
    screen_int_transfer_count                0x00071f3c   Data           1  app_tp_transfer.o(.data)
    screen_int_transfer_buffer_ready         0x00071f3d   Data           1  app_tp_transfer.o(.data)
    .data                                    0x00071f4d   Section       40  app_tp_st_touch.o(.data)
    s_calibration_flag                       0x00071f4d   Data           1  app_tp_st_touch.o(.data)
    s_calibration_correct_flag               0x00071f4e   Data           1  app_tp_st_touch.o(.data)
    .data                                    0x00071f78   Section        8  hal_dsi_rx_ctrl.o(.data)
    g_hw_auto_filter                         0x00071f78   Data           1  hal_dsi_rx_ctrl.o(.data)
    g_esc_clk                                0x00071f7c   Data           4  hal_dsi_rx_ctrl.o(.data)
    .data                                    0x00071f80   Section        3  hal_dsi_tx_ctrl.o(.data)
    g_tx_vcom_en                             0x00071f80   Data           1  hal_dsi_tx_ctrl.o(.data)
    g_tx_vpg_en                              0x00071f81   Data           1  hal_dsi_tx_ctrl.o(.data)
    g_tx_mode                                0x00071f82   Data           1  hal_dsi_tx_ctrl.o(.data)
    .data                                    0x00071f83   Section        1  hal_i2c_master.o(.data)
    s_i2c_m_transfer_end                     0x00071f83   Data           1  hal_i2c_master.o(.data)
    .data                                    0x00071f84   Section       32  hal_i2c_slave.o(.data)
    s_txbuffer_complate                      0x00071f84   Data           1  hal_i2c_slave.o(.data)
    s_i2c_s_dma_end                          0x00071f85   Data           1  hal_i2c_slave.o(.data)
    s_i2c_s_receive_cnt                      0x00071f86   Data           1  hal_i2c_slave.o(.data)
    sg_i2c_s_index                           0x00071f87   Data           1  hal_i2c_slave.o(.data)
    s_hal_slave_rxbuffer                     0x00071f88   Data           4  hal_i2c_slave.o(.data)
    s_hal_slave_rxbuffer_size                0x00071f8c   Data           4  hal_i2c_slave.o(.data)
    hal_i2c_s_callback                       0x00071f90   Data           4  hal_i2c_slave.o(.data)
    sg_tx_byte_num                           0x00071f94   Data           4  hal_i2c_slave.o(.data)
    s_receive_count                          0x00071f98   Data           4  hal_i2c_slave.o(.data)
    s_tx_buffer_t                            0x00071f9c   Data           4  hal_i2c_slave.o(.data)
    tx_sum                                   0x00071fa0   Data           4  hal_i2c_slave.o(.data)
    .data                                    0x00071fa4   Section      228  app_tp_for_custom_s8.o(.data)
    app_tp_count                             0x00071fae   Data           1  app_tp_for_custom_s8.o(.data)
    phone_85_flag                            0x00071faf   Data           1  app_tp_for_custom_s8.o(.data)
    phone_F6_flag                            0x00071fb0   Data           1  app_tp_for_custom_s8.o(.data)
    phone_E4_flag                            0x00071fb1   Data           1  app_tp_for_custom_s8.o(.data)
    phone_72_flag                            0x00071fb2   Data           1  app_tp_for_custom_s8.o(.data)
    phone_75_flag                            0x00071fb3   Data           1  app_tp_for_custom_s8.o(.data)
    phone_92_flag                            0x00071fb4   Data           1  app_tp_for_custom_s8.o(.data)
    phone_74_flag                            0x00071fb5   Data           1  app_tp_for_custom_s8.o(.data)
    u16CoordY                                0x00071fb8   Data           2  app_tp_for_custom_s8.o(.data)
    u16CoordX                                0x00071fba   Data           2  app_tp_for_custom_s8.o(.data)
    u16CoordY_back                           0x00071fbc   Data           2  app_tp_for_custom_s8.o(.data)
    u16CoordX_back                           0x00071fbe   Data           2  app_tp_for_custom_s8.o(.data)
    .data                                    0x00072088   Section        1  app_tp_for_custom_s8.o(.data)
    .data                                    0x00072089   Section        1  app_tp_for_custom_s8.o(.data)
    .data                                    0x0007208a   Section        1  app_tp_for_custom_s8.o(.data)
    .data                                    0x0007208b   Section        3  app_tp_for_custom_s8.o(.data)
    .data                                    0x0007208e   Section        5  app_tp_for_custom_s8.o(.data)
    .data                                    0x00072094   Section       48  app_tp_for_custom_s8.o(.data)
    .data                                    0x000720c4   Section       24  hal_internal_vsync.o(.data)
    sg_cmd_mode_tx_start                     0x000720c4   Data           1  hal_internal_vsync.o(.data)
    sg_cur_te_info                           0x000720c8   Data           4  hal_internal_vsync.o(.data)
    g_cus_rx_write_cmd_handle                0x000720d0   Data          12  hal_internal_vsync.o(.data)
    .data                                    0x000720dc   Section       12  drv_common.o(.data)
    s_my_tick                                0x000720dc   Data           4  drv_common.o(.data)
    .data                                    0x000720e8   Section        4  drv_gpio.o(.data)
    g_ap_reset_cb                            0x000720e8   Data           4  drv_gpio.o(.data)
    .data                                    0x000720ec   Section        8  drv_i2c_dma.o(.data)
    i2c0_dma_callback                        0x000720ec   Data           4  drv_i2c_dma.o(.data)
    i2c1_dma_callback                        0x000720f0   Data           4  drv_i2c_dma.o(.data)
    .data                                    0x000720f4   Section        4  drv_i2c_master.o(.data)
    i2c1_intr_callback                       0x000720f4   Data           4  drv_i2c_master.o(.data)
    .data                                    0x000720f8   Section        4  drv_i2c_slave.o(.data)
    i2c0_intr_callback                       0x000720f8   Data           4  drv_i2c_slave.o(.data)
    .data                                    0x000720fc   Section     1188  drv_param_init.o(.data)
    .data                                    0x000725a0   Section        4  drv_spi_master.o(.data)
    SPIM_intr_callback                       0x000725a0   Data           4  drv_spi_master.o(.data)
    .data                                    0x000725a4   Section        8  drv_swire.o(.data)
    s_swire_cb                               0x000725a4   Data           8  drv_swire.o(.data)
    .data                                    0x000725ac   Section        1  drv_sys_cfg.o(.data)
    sg_ap_rstn_trigger_type                  0x000725ac   Data           1  drv_sys_cfg.o(.data)
    .data                                    0x000725b0   Section       80  drv_timer.o(.data)
    sg_timer_info                            0x000725b0   Data          80  drv_timer.o(.data)
    .data                                    0x00072600   Section        8  drv_rxbr.o(.data)
    .data                                    0x00072608   Section        4  drv_vidc.o(.data)
    .data                                    0x0007260c   Section        1  drv_phy_common.o(.data)
    g_phy_calibration                        0x0007260c   Data           1  drv_phy_common.o(.data)
    .data                                    0x00072610   Section       12  drv_chip_info.o(.data)
    sg_chip_info                             0x00072610   Data           4  drv_chip_info.o(.data)
    sg_chip_function                         0x00072614   Data           4  drv_chip_info.o(.data)
    sg_chip_encrypt                          0x00072618   Data           4  drv_chip_info.o(.data)
    .data                                    0x0007261c   Section        6  app_tp_enc.o(.data)
    init_flag                                0x0007261c   Data           1  app_tp_enc.o(.data)
    g_u8EncryptFlag                          0x0007261d   Data           1  app_tp_enc.o(.data)
    g_u8EncryptData                          0x0007261e   Data           1  app_tp_enc.o(.data)
    g_u16EncryptCnt                          0x00072620   Data           2  app_tp_enc.o(.data)
    .data                                    0x00072624   Section       18  norflash.o(.data)
    tmprg                                    0x0007262c   Data           4  norflash.o(.data)
    .data                                    0x00072638   Section       12  drv_pwm.o(.data)
    s_pwm_type                               0x00072638   Data           1  drv_pwm.o(.data)
    s_pwm_cb                                 0x0007263c   Data           8  drv_pwm.o(.data)
    .data                                    0x00072644   Section        8  drv_uart.o(.data)
    s_UartFcrReg                             0x00072644   Data           4  drv_uart.o(.data)
    uart_userData                            0x00072648   Data           4  drv_uart.o(.data)
    .data                                    0x0007264c   Section       12  drv_wdg.o(.data)
    sg_wdg_repeat                            0x0007264c   Data           1  drv_wdg.o(.data)
    sg_wdg_cb                                0x00072650   Data           8  drv_wdg.o(.data)
    .data                                    0x00072658   Section        4  stdout.o(.data)
    .data                                    0x0007265c   Section        4  errno.o(.data)
    _errno                                   0x0007265c   Data           4  errno.o(.data)
    .bss                                     0x00072660   Section      400  app_tp_transfer.o(.bss)
    s_screen_read_buffer                     0x00072660   Data         200  app_tp_transfer.o(.bss)
    s_phone_read_buffer                      0x00072728   Data         200  app_tp_transfer.o(.bss)
    .bss                                     0x000727f0   Section       12  app_tp_st_touch.o(.bss)
    .bss                                     0x000727fc   Section      196  hal_dsi_rx_ctrl.o(.bss)
    g_rx_ctrl_handle                         0x000727fc   Data         196  hal_dsi_rx_ctrl.o(.bss)
    .bss                                     0x000728c0   Section       76  hal_dsi_tx_ctrl.o(.bss)
    g_tx_ctrl_handle                         0x000728c0   Data          76  hal_dsi_tx_ctrl.o(.bss)
    .bss                                     0x0007290c   Section      208  hal_uart.o(.bss)
    .bss                                     0x000729dc   Section     2436  hal_internal_vsync.o(.bss)
    g_imm_buffer                             0x00073240   Data         255  hal_internal_vsync.o(.bss)
    sg_te_info                               0x00073340   Data          12  hal_internal_vsync.o(.bss)
    g_imm_packet                             0x0007334c   Data          20  hal_internal_vsync.o(.bss)
    .bss                                     0x00073360   Section       28  drv_dma.o(.bss)
    s_dma_handle                             0x00073360   Data          28  drv_dma.o(.bss)
    .bss                                     0x0007337c   Section       64  drv_gpio.o(.bss)
    s_gpio_cb                                0x0007337c   Data          64  drv_gpio.o(.bss)
    .bss                                     0x000733bc   Section      320  drv_i2c_dma.o(.bss)
    i2c0_dma_slave_handle                    0x000733bc   Data         160  drv_i2c_dma.o(.bss)
    i2c1_dma_master_handle                   0x0007345c   Data         160  drv_i2c_dma.o(.bss)
    .bss                                     0x000734fc   Section     4144  dcs_packet_fifo.o(.bss)
    .bss                                     0x0007452c   Section      256  tau_log.o(.bss)
    .bss                                     0x0007462c   Section       32  hal_spi_slave.o(.bss)
    STACK                                    0x00074650   Section     4096  startup_armcm0.o(STACK)

    Global Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    BuildAttributes$$THM_ISAv3M$S$PE$A:L22$X:L11$S22$IEEE1$IW$USESV6$~STKCKD$USESV7$~SHL$OTIME$ROPI$IEEEJ$EBA8$MICROLIB$REQ8$PRES8$EABIv2 0x00000000   Number         0  anon$$obj.o ABSOLUTE
    __ARM_use_no_argv                        0x00000000   Number         0  main.o ABSOLUTE
    _printf_a                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_c                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_charcount                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_d                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_e                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_f                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_flags                            0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_dec                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_hex                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_g                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_i                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_int_dec                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_l                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ll                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lld                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lli                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llo                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llu                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llx                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_dec                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_hex                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_oct                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ls                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_mbtowc                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_n                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_o                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_p                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_percent                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_pre_padding                      0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_return_value                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_s                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_sizespec                         0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_str                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_signed                  0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_unsigned                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_u                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wctomb                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_widthprec                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_x                                0x00000000   Number         0  stubs.o ABSOLUTE
    __cpp_initialize__aeabi_                  - Undefined Weak Reference
    __cxa_finalize                            - Undefined Weak Reference
    _clock_init                               - Undefined Weak Reference
    _microlib_exit                            - Undefined Weak Reference
    __Vectors_Size                           0x000000c0   Number         0  startup_armcm0.o ABSOLUTE
    __Vectors                                0x00010000   Data           4  startup_armcm0.o(RESET)
    __Vectors_End                            0x000100c0   Data           0  startup_armcm0.o(RESET)
    __main                                   0x000100c1   Thumb Code     0  entry.o(.ARM.Collect$$$$00000000)
    _main_stk                                0x000100c1   Thumb Code     0  entry2.o(.ARM.Collect$$$$00000001)
    _main_scatterload                        0x000100c5   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    __main_after_scatterload                 0x000100c9   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    _main_clock                              0x000100c9   Thumb Code     0  entry7b.o(.ARM.Collect$$$$00000008)
    _main_cpp_init                           0x000100c9   Thumb Code     0  entry8b.o(.ARM.Collect$$$$0000000A)
    _main_init                               0x000100c9   Thumb Code     0  entry9a.o(.ARM.Collect$$$$0000000B)
    __rt_final_cpp                           0x000100d1   Thumb Code     0  entry10a.o(.ARM.Collect$$$$0000000D)
    __rt_final_exit                          0x000100d1   Thumb Code     0  entry11a.o(.ARM.Collect$$$$0000000F)
    Reset_Handler                            0x000100d5   Thumb Code    28  startup_armcm0.o(.text)
    NMI_Handler                              0x000100f1   Thumb Code     2  startup_armcm0.o(.text)
    SVC_Handler                              0x000100f5   Thumb Code     2  startup_armcm0.o(.text)
    PendSV_Handler                           0x000100f7   Thumb Code     2  startup_armcm0.o(.text)
    OTP_IRQn_Handler                         0x00010123   Thumb Code     2  startup_armcm0.o(.text)
    PVD_IRQn_Handler                         0x00010127   Thumb Code     2  startup_armcm0.o(.text)
    __aeabi_uidiv                            0x0001014d   Thumb Code     0  uidiv.o(.text)
    __aeabi_uidivmod                         0x0001014d   Thumb Code    44  uidiv.o(.text)
    __aeabi_idiv                             0x00010179   Thumb Code     0  idiv.o(.text)
    __aeabi_idivmod                          0x00010179   Thumb Code    40  idiv.o(.text)
    __aeabi_memcpy                           0x000101a1   Thumb Code    36  memcpya.o(.text)
    __aeabi_memcpy4                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memcpy8                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memset                           0x000101c5   Thumb Code    14  memseta.o(.text)
    __aeabi_memset4                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memset8                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr                           0x000101d3   Thumb Code     4  memseta.o(.text)
    __aeabi_memclr4                          0x000101d3   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr8                          0x000101d3   Thumb Code     0  memseta.o(.text)
    _memset$wrapper                          0x000101d7   Thumb Code    18  memseta.o(.text)
    __aeabi_fadd                             0x000101e9   Thumb Code   162  fadd.o(.text)
    __aeabi_fsub                             0x0001028b   Thumb Code     8  fadd.o(.text)
    __aeabi_frsub                            0x00010293   Thumb Code     8  fadd.o(.text)
    __aeabi_fmul                             0x0001029b   Thumb Code   122  fmul.o(.text)
    __aeabi_fdiv                             0x00010315   Thumb Code   124  fdiv.o(.text)
    __ARM_scalbnf                            0x00010391   Thumb Code    24  fscalb.o(.text)
    scalbnf                                  0x00010391   Thumb Code     0  fscalb.o(.text)
    __aeabi_dadd                             0x000103a9   Thumb Code   328  dadd.o(.text)
    __aeabi_dsub                             0x000104f1   Thumb Code    12  dadd.o(.text)
    __aeabi_drsub                            0x000104fd   Thumb Code    12  dadd.o(.text)
    __aeabi_dmul                             0x0001050d   Thumb Code   202  dmul.o(.text)
    __aeabi_ddiv                             0x000105dd   Thumb Code   234  ddiv.o(.text)
    __aeabi_i2f                              0x000106cd   Thumb Code    22  fflti.o(.text)
    __aeabi_ui2f                             0x000106e3   Thumb Code    14  ffltui.o(.text)
    __aeabi_ui2d                             0x000106f1   Thumb Code    24  dfltui.o(.text)
    __aeabi_f2iz                             0x0001070d   Thumb Code    50  ffixi.o(.text)
    __aeabi_f2uiz                            0x0001073f   Thumb Code    40  ffixui.o(.text)
    __aeabi_d2iz                             0x00010769   Thumb Code    62  dfixi.o(.text)
    __aeabi_d2uiz                            0x000107b1   Thumb Code    50  dfixui.o(.text)
    __aeabi_f2d                              0x000107ed   Thumb Code    40  f2d.o(.text)
    __aeabi_cdcmpeq                          0x00010815   Thumb Code     0  cdcmple.o(.text)
    __aeabi_cdcmple                          0x00010815   Thumb Code    38  cdcmple.o(.text)
    __aeabi_cfrcmple                         0x0001083d   Thumb Code    20  cfrcmple.o(.text)
    __aeabi_uldivmod                         0x00010851   Thumb Code    96  uldiv.o(.text)
    __aeabi_llsl                             0x000108b1   Thumb Code    32  llshl.o(.text)
    _ll_shift_l                              0x000108b1   Thumb Code     0  llshl.o(.text)
    __aeabi_llsr                             0x000108d1   Thumb Code    34  llushr.o(.text)
    _ll_ushift_r                             0x000108d1   Thumb Code     0  llushr.o(.text)
    __aeabi_lasr                             0x000108f3   Thumb Code    38  llsshr.o(.text)
    _ll_sshift_r                             0x000108f3   Thumb Code     0  llsshr.o(.text)
    __I$use$fp                               0x00010919   Thumb Code     0  iusefp.o(.text)
    _float_round                             0x00010919   Thumb Code    16  fepilogue.o(.text)
    _float_epilogue                          0x00010929   Thumb Code   114  fepilogue.o(.text)
    _double_round                            0x0001099b   Thumb Code    26  depilogue.o(.text)
    _double_epilogue                         0x000109b5   Thumb Code   164  depilogue.o(.text)
    _dsqrt                                   0x00010a59   Thumb Code   162  dsqrt.o(.text)
    __aeabi_d2ulz                            0x00010afd   Thumb Code    54  dfixul.o(.text)
    __aeabi_cdrcmple                         0x00010b3d   Thumb Code    38  cdrcmple.o(.text)
    __scatterload                            0x00010b65   Thumb Code    28  init.o(.text)
    __scatterload_rt2                        0x00010b65   Thumb Code     0  init.o(.text)
    __decompress                             0x00010b89   Thumb Code     0  __dczerorl2.o(.text)
    __decompress1                            0x00010b89   Thumb Code    86  __dczerorl2.o(.text)
    ADC_IRQn_Handler                         0x00010be1   Thumb Code    18  irq_redirect .o(i.ADC_IRQn_Handler)
    AP_NRESET_IRQn_Handler                   0x00010bf9   Thumb Code    18  irq_redirect .o(i.AP_NRESET_IRQn_Handler)
    DMA_IRQn_Handler                         0x00010c11   Thumb Code    14  irq_redirect .o(i.DMA_IRQn_Handler)
    EXTI_INT0_IRQn_Handler                   0x00010c25   Thumb Code    22  irq_redirect .o(i.EXTI_INT0_IRQn_Handler)
    EXTI_INT1_IRQn_Handler                   0x00010c41   Thumb Code    22  irq_redirect .o(i.EXTI_INT1_IRQn_Handler)
    EXTI_INT2_IRQn_Handler                   0x00010c5d   Thumb Code    22  irq_redirect .o(i.EXTI_INT2_IRQn_Handler)
    EXTI_INT3_IRQn_Handler                   0x00010c79   Thumb Code    22  irq_redirect .o(i.EXTI_INT3_IRQn_Handler)
    EXTI_INT4_IRQn_Handler                   0x00010c95   Thumb Code    22  irq_redirect .o(i.EXTI_INT4_IRQn_Handler)
    EXTI_INT5_IRQn_Handler                   0x00010cb1   Thumb Code    22  irq_redirect .o(i.EXTI_INT5_IRQn_Handler)
    EXTI_INT6_IRQn_Handler                   0x00010ccd   Thumb Code    22  irq_redirect .o(i.EXTI_INT6_IRQn_Handler)
    EXTI_INT7_IRQn_Handler                   0x00010ce9   Thumb Code    22  irq_redirect .o(i.EXTI_INT7_IRQn_Handler)
    EncryptCheck                             0x00010d05   Thumb Code    90  app_tp_enc.o(i.EncryptCheck)
    FLSCTRL_IRQn_Handler                     0x00010d69   Thumb Code    14  irq_redirect .o(i.FLSCTRL_IRQn_Handler)
    Gpio_swire_output                        0x00010d7d   Thumb Code   110  ap_demo.o(i.Gpio_swire_output)
    HardFault_Handler                        0x00010df1   Thumb Code    14  irq_redirect .o(i.HardFault_Handler)
    I2C0_IRQn_Handler                        0x00010e05   Thumb Code    18  irq_redirect .o(i.I2C0_IRQn_Handler)
    I2C1_IRQn_Handler                        0x00010e1d   Thumb Code    18  irq_redirect .o(i.I2C1_IRQn_Handler)
    LCDC_IRQn_Handler                        0x00010e35   Thumb Code    18  irq_redirect .o(i.LCDC_IRQn_Handler)
    LOG_printf                               0x00010e4d   Thumb Code    30  tau_log.o(i.LOG_printf)
    MEMC_IRQn_Handler                        0x00010e75   Thumb Code    18  irq_redirect .o(i.MEMC_IRQn_Handler)
    MIPI_RX_IRQn_Handler                     0x00010e8d   Thumb Code    18  irq_redirect .o(i.MIPI_RX_IRQn_Handler)
    MIPI_TX_IRQn_Handler                     0x00010ea5   Thumb Code    18  irq_redirect .o(i.MIPI_TX_IRQn_Handler)
    PWMDET_IRQn_Handler                      0x00010ebd   Thumb Code    22  irq_redirect .o(i.PWMDET_IRQn_Handler)
    SPIM_IRQn_Handler                        0x00010ed9   Thumb Code    22  irq_redirect .o(i.SPIM_IRQn_Handler)
    SPIS_IRQn_Handler                        0x00010ef5   Thumb Code    22  irq_redirect .o(i.SPIS_IRQn_Handler)
    SWIRE_IRQn_Handler                       0x00010f11   Thumb Code    22  irq_redirect .o(i.SWIRE_IRQn_Handler)
    SysTick_Handler                          0x00010f2d   Thumb Code    18  irq_redirect .o(i.SysTick_Handler)
    TIMER0_IRQn_Handler                      0x00010f45   Thumb Code    18  irq_redirect .o(i.TIMER0_IRQn_Handler)
    TIMER1_IRQn_Handler                      0x00010f5d   Thumb Code    18  irq_redirect .o(i.TIMER1_IRQn_Handler)
    TIMER2_IRQn_Handler                      0x00010f75   Thumb Code    18  irq_redirect .o(i.TIMER2_IRQn_Handler)
    TIMER3_IRQn_Handler                      0x00010f8d   Thumb Code    18  irq_redirect .o(i.TIMER3_IRQn_Handler)
    UART0_IRQ_Handle                         0x00010fa5   Thumb Code    20  drv_uart.o(i.UART0_IRQ_Handle)
    UART_DisableDma                          0x00010fc1   Thumb Code     2  drv_uart.o(i.UART_DisableDma)
    UART_GetInstance                         0x00010fc3   Thumb Code     4  drv_uart.o(i.UART_GetInstance)
    UART_IRQn_Handler                        0x00010fc9   Thumb Code    18  irq_redirect .o(i.UART_IRQn_Handler)
    UART_SwitchSCLK                          0x00010fe1   Thumb Code    26  drv_uart.o(i.UART_SwitchSCLK)
    __scatterload_null                       0x00010ffb   Thumb Code     2  handlers.o(i.__scatterload_null)
    drv_dsi_rx_set_inten                     0x00010ffd   Thumb Code     4  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    s_RAM_CK                                 0x00011000   Data          20  drv_common.o(.ARM.__at_0x11000)
    drv_dsi_tx_command_put_payload           0x00011015   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    s_debug_state                            0x00011018   Data           4  drv_common.o(.ARM.__at_0x11018)
    S20_Start_init                           0x0001101d   Thumb Code   300  app_tp_transfer.o(i.S20_Start_init)
    UART_ResetRxFIFO                         0x00011161   Thumb Code    32  drv_uart.o(i.UART_ResetRxFIFO)
    UART_SetBaudRate                         0x00011185   Thumb Code    72  drv_uart.o(i.UART_SetBaudRate)
    UART_TransferHandleIRQ                   0x000111cd   Thumb Code   308  drv_uart.o(i.UART_TransferHandleIRQ)
    UART_WriteBlocking                       0x00011301   Thumb Code    26  drv_uart.o(i.UART_WriteBlocking)
    UART_init                                0x0001131d   Thumb Code   182  drv_uart.o(i.UART_init)
    VIDC_IRQn_Handler                        0x000113d9   Thumb Code    18  irq_redirect .o(i.VIDC_IRQn_Handler)
    VPRE_IRQn_Handler                        0x000113f1   Thumb Code    18  irq_redirect .o(i.VPRE_IRQn_Handler)
    WDG_IRQn_Handler                         0x00011409   Thumb Code    18  irq_redirect .o(i.WDG_IRQn_Handler)
    __0printf                                0x00011421   Thumb Code    24  printfa.o(i.__0printf)
    __1printf                                0x00011421   Thumb Code     0  printfa.o(i.__0printf)
    __2printf                                0x00011421   Thumb Code     0  printfa.o(i.__0printf)
    __c89printf                              0x00011421   Thumb Code     0  printfa.o(i.__0printf)
    printf                                   0x00011421   Thumb Code     0  printfa.o(i.__0printf)
    __0vsprintf                              0x00011441   Thumb Code    30  printfa.o(i.__0vsprintf)
    __1vsprintf                              0x00011441   Thumb Code     0  printfa.o(i.__0vsprintf)
    __2vsprintf                              0x00011441   Thumb Code     0  printfa.o(i.__0vsprintf)
    __c89vsprintf                            0x00011441   Thumb Code     0  printfa.o(i.__0vsprintf)
    vsprintf                                 0x00011441   Thumb Code     0  printfa.o(i.__0vsprintf)
    __ARM_clz                                0x00011465   Thumb Code    46  depilogue.o(i.__ARM_clz)
    __ARM_common_switch8                     0x00011493   Thumb Code    26  ap_demo.o(i.__ARM_common_switch8)
    __scatterload_copy                       0x00011559   Thumb Code    14  handlers.o(i.__scatterload_copy)
    __scatterload_zeroinit                   0x00011567   Thumb Code    14  handlers.o(i.__scatterload_zeroinit)
    __set_errno                              0x00011575   Thumb Code     6  errno.o(i.__set_errno)
    ap_demo                                  0x00012e95   Thumb Code   292  ap_demo.o(i.ap_demo)
    ap_get_tp_calibration_status_01          0x000130a5   Thumb Code    28  app_tp_st_touch.o(i.ap_get_tp_calibration_status_01)
    ap_tp_st_touch_calibration               0x0001343d   Thumb Code   170  app_tp_st_touch.o(i.ap_tp_st_touch_calibration)
    ap_tp_st_touch_error_handler_F3          0x000134ed   Thumb Code    26  app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_F3)
    ap_tp_st_touch_error_handler_FF          0x00013507   Thumb Code    32  app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_FF)
    ap_tp_st_touch_get_calibration_success_mark 0x00013529   Thumb Code   150  app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark)
    ap_tp_st_touch_scan_point_init           0x000135d1   Thumb Code    24  app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init)
    ap_tp_st_touch_scan_point_record_event   0x000135ed   Thumb Code   142  app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event)
    ap_tp_st_touch_scan_point_record_event_exec 0x00013681   Thumb Code    44  app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec)
    ap_tp_st_touch_simulate_finger_release_event 0x000136b5   Thumb Code    44  app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event)
    ap_tp_st_touch_software_reset            0x000136e9   Thumb Code   106  app_tp_st_touch.o(i.ap_tp_st_touch_software_reset)
    app_ADC_IRQn_Handler                     0x00013785   Thumb Code    22  drv_rxbr.o(i.app_ADC_IRQn_Handler)
    app_AP_NRESET_IRQn_Handler               0x000137a1   Thumb Code    32  drv_gpio.o(i.app_AP_NRESET_IRQn_Handler)
    app_EXTI_INT0_IRQn_Handler               0x000137c5   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler)
    app_EXTI_INT1_IRQn_Handler               0x000137e1   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler)
    app_EXTI_INT2_IRQn_Handler               0x000137fd   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler)
    app_EXTI_INT3_IRQn_Handler               0x00013819   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler)
    app_EXTI_INT4_IRQn_Handler               0x00013835   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler)
    app_EXTI_INT5_IRQn_Handler               0x00013851   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler)
    app_EXTI_INT6_IRQn_Handler               0x0001386d   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler)
    app_EXTI_INT7_IRQn_Handler               0x00013889   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler)
    app_HardFault_Handler                    0x000138a5   Thumb Code    12  drv_common.o(i.app_HardFault_Handler)
    app_I2C0_IRQn_Handler                    0x000138ed   Thumb Code    14  drv_i2c_slave.o(i.app_I2C0_IRQn_Handler)
    app_I2C1_IRQn_Handler                    0x00013905   Thumb Code     8  drv_i2c_master.o(i.app_I2C1_IRQn_Handler)
    app_LCDC_IRQn_Handler                    0x00013915   Thumb Code   208  hal_internal_vsync.o(i.app_LCDC_IRQn_Handler)
    app_MEMC_IRQn_Handler                    0x00013ab9   Thumb Code   132  drv_memc.o(i.app_MEMC_IRQn_Handler)
    app_MIPI_RX_IRQn_Handler                 0x00013b41   Thumb Code   232  drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler)
    app_MIPI_TX_IRQn_Handler                 0x00013dd9   Thumb Code    56  drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler)
    app_PWMDET_IRQn_Handler                  0x00013e79   Thumb Code    62  drv_pwm.o(i.app_PWMDET_IRQn_Handler)
    app_SPIM_IRQn_Handler                    0x00013ec1   Thumb Code    34  drv_spi_master.o(i.app_SPIM_IRQn_Handler)
    app_SPIS_IRQn_Handler                    0x00013ef1   Thumb Code   500  hal_spi_slave.o(i.app_SPIS_IRQn_Handler)
    app_SWIRE_IRQn_Handler                   0x000140f1   Thumb Code    28  drv_swire.o(i.app_SWIRE_IRQn_Handler)
    app_SysTick_Handler                      0x00014111   Thumb Code    20  drv_common.o(i.app_SysTick_Handler)
    app_TIMER0_IRQn_Handler                  0x00014129   Thumb Code    10  drv_timer.o(i.app_TIMER0_IRQn_Handler)
    app_TIMER1_IRQn_Handler                  0x00014133   Thumb Code    10  drv_timer.o(i.app_TIMER1_IRQn_Handler)
    app_TIMER2_IRQn_Handler                  0x0001413d   Thumb Code    10  drv_timer.o(i.app_TIMER2_IRQn_Handler)
    app_TIMER3_IRQn_Handler                  0x00014147   Thumb Code    10  drv_timer.o(i.app_TIMER3_IRQn_Handler)
    app_UART_IRQn_Handler                    0x00014151   Thumb Code     8  drv_uart.o(i.app_UART_IRQn_Handler)
    app_VIDC_IRQn_Handler                    0x00014159   Thumb Code    22  drv_vidc.o(i.app_VIDC_IRQn_Handler)
    app_VPRE_IRQn_Handler                    0x00014175   Thumb Code    22  drv_rxbr.o(i.app_VPRE_IRQn_Handler)
    app_WDG_IRQn_Handler                     0x00014191   Thumb Code    52  drv_wdg.o(i.app_WDG_IRQn_Handler)
    app_dma_irq_handler                      0x000141c9   Thumb Code    10  drv_dma.o(i.app_dma_irq_handler)
    app_fls_ctrl_Handler                     0x000141d9   Thumb Code    38  norflash.o(i.app_fls_ctrl_Handler)
    app_tp_I2C_init                          0x00014209   Thumb Code    26  app_tp_transfer.o(i.app_tp_I2C_init)
    app_tp_calibration_exec                  0x0001422d   Thumb Code    50  app_tp_st_touch.o(i.app_tp_calibration_exec)
    app_tp_init                              0x00014295   Thumb Code    56  app_tp_transfer.o(i.app_tp_init)
    app_tp_m_read                            0x000142d9   Thumb Code    32  app_tp_transfer.o(i.app_tp_m_read)
    app_tp_m_write                           0x000142f9   Thumb Code     8  app_tp_transfer.o(i.app_tp_m_write)
    app_tp_phone_analysis_data               0x00014301   Thumb Code   992  app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data)
    app_tp_phone_clear_reset_on              0x0001471d   Thumb Code     8  app_tp_transfer.o(i.app_tp_phone_clear_reset_on)
    app_tp_s_read                            0x00014729   Thumb Code     8  app_tp_transfer.o(i.app_tp_s_read)
    app_tp_s_write                           0x00014731   Thumb Code     8  app_tp_transfer.o(i.app_tp_s_write)
    app_tp_screen_analysis_int               0x00014739   Thumb Code   718  app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int)
    app_tp_screen_init                       0x00014a15   Thumb Code    42  app_tp_transfer.o(i.app_tp_screen_init)
    app_tp_transfer_screen_int               0x00014a91   Thumb Code   336  app_tp_transfer.o(i.app_tp_transfer_screen_int)
    app_tp_transfer_screen_start             0x00014bf1   Thumb Code    18  app_tp_transfer.o(i.app_tp_transfer_screen_start)
    blue_change_ccm                          0x00014c09   Thumb Code    54  ap_demo.o(i.blue_change_ccm)
    board_Init                               0x00014c41   Thumb Code    30  board.o(i.board_Init)
    calc_framebuffer_setting                 0x00014c65   Thumb Code  1258  hal_internal_vsync.o(i.calc_framebuffer_setting)
    ceil                                     0x00015155   Thumb Code   180  ceil.o(i.ceil)
    dcs_packet_fifo_alloc                    0x000152d9   Thumb Code    80  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    dcs_packet_fifo_init                     0x00015331   Thumb Code    18  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    dcs_packet_free_fifo_header              0x00015349   Thumb Code    60  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    dcs_packet_get_fifo_header               0x0001538d   Thumb Code    26  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    delayMs                                  0x000153dd   Thumb Code    24  tau_delay.o(i.delayMs)
    delayUs                                  0x000153f5   Thumb Code    34  tau_delay.o(i.delayUs)
    drv_ap_rst_trig_edge_detect              0x00015471   Thumb Code    46  drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect)
    drv_chip_info_get_info                   0x000154a9   Thumb Code     6  drv_chip_info.o(i.drv_chip_info_get_info)
    drv_chip_info_init                       0x000154b5   Thumb Code    56  drv_chip_info.o(i.drv_chip_info_init)
    drv_chip_rx_info_check                   0x000154f5   Thumb Code    98  drv_chip_info.o(i.drv_chip_rx_info_check)
    drv_chip_rx_init_done                    0x000155a5   Thumb Code    16  drv_chip_info.o(i.drv_chip_rx_init_done)
    drv_common_enable_systick                0x000155b9   Thumb Code    70  drv_common.o(i.drv_common_enable_systick)
    drv_common_system_init                   0x00015611   Thumb Code     8  drv_common.o(i.drv_common_system_init)
    drv_crgu_config_reset_modules            0x00015619   Thumb Code    10  drv_crgu.o(i.drv_crgu_config_reset_modules)
    drv_crgu_set_ahb_pre_div                 0x00015629   Thumb Code    14  drv_crgu.o(i.drv_crgu_set_ahb_pre_div)
    drv_crgu_set_ahb_src                     0x0001563d   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_ahb_src)
    drv_crgu_set_clock                       0x00015651   Thumb Code    26  drv_crgu.o(i.drv_crgu_set_clock)
    drv_crgu_set_dpi_mux_src                 0x00015671   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dpi_mux_src)
    drv_crgu_set_dpi_pre_div                 0x00015685   Thumb Code    18  drv_crgu.o(i.drv_crgu_set_dpi_pre_div)
    drv_crgu_set_dpi_pre_src                 0x0001569d   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dpi_pre_src)
    drv_crgu_set_dsc_core_div                0x000156b1   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dsc_core_div)
    drv_crgu_set_dsco_src                    0x000156c5   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dsco_src)
    drv_crgu_set_dsco_src_div                0x000156d9   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dsco_src_div)
    drv_crgu_set_fb_div                      0x000156ed   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_fb_div)
    drv_crgu_set_fb_src                      0x00015701   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_fb_src)
    drv_crgu_set_lcdc_div                    0x00015715   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_lcdc_div)
    drv_crgu_set_lcdc_src                    0x00015729   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_lcdc_src)
    drv_crgu_set_mipi_cfg_src                0x0001573d   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_mipi_cfg_src)
    drv_crgu_set_mipi_ref_src                0x00015751   Thumb Code    18  drv_crgu.o(i.drv_crgu_set_mipi_ref_src)
    drv_crgu_set_reset                       0x00015769   Thumb Code    20  drv_crgu.o(i.drv_crgu_set_reset)
    drv_crgu_set_rxbr_div                    0x00015781   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_rxbr_div)
    drv_crgu_set_rxbr_src                    0x00015795   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_rxbr_src)
    drv_crgu_set_vidc_src                    0x000157a9   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_vidc_src)
    drv_dma_clear_flag                       0x000157bd   Thumb Code    24  drv_dma.o(i.drv_dma_clear_flag)
    drv_dma_create_handle                    0x000157d5   Thumb Code    22  drv_dma.o(i.drv_dma_create_handle)
    drv_dma_disenable_channel                0x000157f1   Thumb Code    16  drv_dma.o(i.drv_dma_disenable_channel)
    drv_dma_enable_channel                   0x00015801   Thumb Code    16  drv_dma.o(i.drv_dma_enable_channel)
    drv_dma_enable_channel_interrupts        0x00015811   Thumb Code    32  drv_dma.o(i.drv_dma_enable_channel_interrupts)
    drv_dma_get_channel_flag                 0x00015835   Thumb Code    12  drv_dma.o(i.drv_dma_get_channel_flag)
    drv_dma_irq_handler                      0x00015841   Thumb Code   138  drv_dma.o(i.drv_dma_irq_handler)
    drv_dma_prepar_transfer                  0x000158d1   Thumb Code    18  drv_dma.o(i.drv_dma_prepar_transfer)
    drv_dma_set_burst                        0x000158e3   Thumb Code    26  drv_dma.o(i.drv_dma_set_burst)
    drv_dma_set_callback                     0x000158fd   Thumb Code     6  drv_dma.o(i.drv_dma_set_callback)
    drv_dma_set_transfer                     0x00015905   Thumb Code    62  drv_dma.o(i.drv_dma_set_transfer)
    drv_dsc_dec_convert_pps_rc_parameter     0x00015949   Thumb Code    54  drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter)
    drv_dsc_dec_disable                      0x0001597f   Thumb Code    12  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    drv_dsc_dec_enable                       0x0001598d   Thumb Code    88  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    drv_dsc_dec_get_nslc                     0x00015a01   Thumb Code    10  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    drv_dsc_dec_set_u8_pps                   0x00015a0b   Thumb Code    40  drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps)
    drv_dsi_rx_calc_ipi_tx_delay             0x00015a35   Thumb Code   244  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    drv_dsi_rx_enable_irq                    0x00015b39   Thumb Code    58  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    drv_dsi_rx_get_compression_en            0x00015be5   Thumb Code     8  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    drv_dsi_rx_get_max_ret_size              0x00015bed   Thumb Code     6  drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size)
    drv_dsi_rx_power_up                      0x00015bf3   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    drv_dsi_rx_set_ctrl_cfg                  0x00015c01   Thumb Code    32  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    drv_dsi_rx_set_ddi_cfg                   0x00015c21   Thumb Code    16  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    drv_dsi_rx_set_ipi_cfg                   0x00015c31   Thumb Code    16  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    drv_dsi_rx_set_lane_swap                 0x00015c41   Thumb Code    70  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    drv_dsi_rx_set_resp_cnt                  0x00015c87   Thumb Code    38  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    drv_dsi_rx_set_up_phy                    0x00015cad   Thumb Code   256  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    drv_dsi_rx_shut_down                     0x00015db1   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    drv_dsi_tx_command_header                0x00015dbf   Thumb Code    20  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    drv_dsi_tx_command_mode_cfg              0x00015dd3   Thumb Code   108  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    drv_dsi_tx_config_eotp                   0x00015e3f   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    drv_dsi_tx_config_int                    0x00015e57   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    drv_dsi_tx_dpi_lpcmd_time                0x00015e5f   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    drv_dsi_tx_dpi_mode                      0x00015e67   Thumb Code    10  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    drv_dsi_tx_dpi_polarity                  0x00015e71   Thumb Code    36  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    drv_dsi_tx_edpi_cmd_size                 0x00015e95   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    drv_dsi_tx_get_cmd_status                0x00015e99   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    drv_dsi_tx_mode                          0x00015e9d   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    drv_dsi_tx_phy_clock_lane_auto_lp        0x00015ea1   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    drv_dsi_tx_phy_clock_lane_req_hs         0x00015eb9   Thumb Code    26  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    drv_dsi_tx_phy_lane_mode                 0x00015ed3   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    drv_dsi_tx_phy_status_ready              0x00015edf   Thumb Code   100  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    drv_dsi_tx_phy_status_stopstate          0x00015f43   Thumb Code    62  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    drv_dsi_tx_phy_test_setup                0x00015f81   Thumb Code   308  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    drv_dsi_tx_phy_time_cfg                  0x000160b5   Thumb Code    30  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    drv_dsi_tx_powerup                       0x000160d3   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    drv_dsi_tx_response_mode                 0x000160db   Thumb Code    28  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    drv_dsi_tx_set_bta_ack                   0x000160f7   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    drv_dsi_tx_set_esc_div                   0x0001610f   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    drv_dsi_tx_set_int                       0x0001611d   Thumb Code    58  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    drv_dsi_tx_set_time_out_div              0x0001615d   Thumb Code    16  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    drv_dsi_tx_set_video_chunk               0x0001616d   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    drv_dsi_tx_set_video_timing              0x00016175   Thumb Code    34  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    drv_dsi_tx_shutdown                      0x00016197   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    drv_dsi_tx_timeout_cfg                   0x0001619f   Thumb Code    38  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    drv_dsi_tx_video_mode_cfg                0x000161c5   Thumb Code   170  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    drv_dsi_tx_video_mode_disable_hact_cmd   0x0001626f   Thumb Code    22  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_disable_hact_cmd)
    drv_dsi_tx_video_mode_set_lp_cmd         0x00016285   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd)
    drv_efuse_enter_inactive                 0x0001629d   Thumb Code    46  drv_efuse.o(i.drv_efuse_enter_inactive)
    drv_efuse_int_enable                     0x000162cb   Thumb Code    12  drv_efuse.o(i.drv_efuse_int_enable)
    drv_efuse_read                           0x000162d7   Thumb Code    50  drv_efuse.o(i.drv_efuse_read)
    drv_efuse_read_req                       0x00016309   Thumb Code    24  drv_efuse.o(i.drv_efuse_read_req)
    drv_gpio_get_input_data                  0x00016321   Thumb Code    20  drv_gpio.o(i.drv_gpio_get_input_data)
    drv_gpio_register_ap_reset_callback      0x00016339   Thumb Code     6  drv_gpio.o(i.drv_gpio_register_ap_reset_callback)
    drv_gpio_register_callback               0x00016345   Thumb Code    14  drv_gpio.o(i.drv_gpio_register_callback)
    drv_gpio_set_int                         0x00016359   Thumb Code    74  drv_gpio.o(i.drv_gpio_set_int)
    drv_gpio_set_ioe                         0x000163a9   Thumb Code    26  drv_gpio.o(i.drv_gpio_set_ioe)
    drv_gpio_set_mode0                       0x000163c9   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode0)
    drv_gpio_set_mode1                       0x000163d9   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode1)
    drv_gpio_set_mode2                       0x000163e9   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode2)
    drv_gpio_set_mode3                       0x000163f9   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode3)
    drv_gpio_set_pull_state                  0x00016429   Thumb Code   298  drv_gpio.o(i.drv_gpio_set_pull_state)
    drv_i2c0_set_callback                    0x00016559   Thumb Code     6  drv_i2c_slave.o(i.drv_i2c0_set_callback)
    drv_i2c1_set_callback                    0x00016565   Thumb Code     6  drv_i2c_master.o(i.drv_i2c1_set_callback)
    drv_i2c_dma_init                         0x000165a5   Thumb Code   146  drv_i2c_dma.o(i.drv_i2c_dma_init)
    drv_i2c_enable_rx_dma                    0x00016651   Thumb Code    26  drv_i2c_dma.o(i.drv_i2c_enable_rx_dma)
    drv_i2c_enable_tx_dma                    0x0001666b   Thumb Code    24  drv_i2c_dma.o(i.drv_i2c_enable_tx_dma)
    drv_i2c_m_clear_it_pending_bit           0x00016685   Thumb Code    86  drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit)
    drv_i2c_m_enable                         0x000166e5   Thumb Code    10  drv_i2c_master.o(i.drv_i2c_m_enable)
    drv_i2c_m_enable_intr                    0x000166f5   Thumb Code    42  drv_i2c_master.o(i.drv_i2c_m_enable_intr)
    drv_i2c_master_init                      0x0001672d   Thumb Code   118  drv_i2c_master.o(i.drv_i2c_master_init)
    drv_i2c_master_read_dma                  0x000167b9   Thumb Code    82  drv_i2c_dma.o(i.drv_i2c_master_read_dma)
    drv_i2c_master_write_dma                 0x00016815   Thumb Code    50  drv_i2c_dma.o(i.drv_i2c_master_write_dma)
    drv_i2c_s_clear_it_pending_bit           0x0001688f   Thumb Code    66  drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit)
    drv_i2c_s_config_intr                    0x000168d1   Thumb Code     4  drv_i2c_slave.o(i.drv_i2c_s_config_intr)
    drv_i2c_s_enable                         0x000168d5   Thumb Code     8  drv_i2c_slave.o(i.drv_i2c_s_enable)
    drv_i2c_s_get_fifo_status                0x000168dd   Thumb Code    20  drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status)
    drv_i2c_s_set_intr                       0x000168f1   Thumb Code    74  drv_i2c_slave.o(i.drv_i2c_s_set_intr)
    drv_i2c_s_write_data                     0x00016941   Thumb Code    28  drv_i2c_slave.o(i.drv_i2c_s_write_data)
    drv_i2c_set_dma_irq_callback             0x0001695d   Thumb Code    68  drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback)
    drv_i2c_slave_init                       0x000169b5   Thumb Code    50  drv_i2c_slave.o(i.drv_i2c_slave_init)
    drv_i2c_slave_write_dma                  0x000169e9   Thumb Code    20  drv_i2c_dma.o(i.drv_i2c_slave_write_dma)
    drv_lcdc_config_bypass                   0x00016a01   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_config_bypass)
    drv_lcdc_config_ccm                      0x00016a19   Thumb Code    48  drv_lcdc.o(i.drv_lcdc_config_ccm)
    drv_lcdc_config_disp_mode                0x00016a49   Thumb Code    22  drv_lcdc.o(i.drv_lcdc_config_disp_mode)
    drv_lcdc_config_dpi_polarity             0x00016a5f   Thumb Code    36  drv_lcdc.o(i.drv_lcdc_config_dpi_polarity)
    drv_lcdc_config_dpi_timing               0x00016a83   Thumb Code    38  drv_lcdc.o(i.drv_lcdc_config_dpi_timing)
    drv_lcdc_config_edpi_mode                0x00016aa9   Thumb Code    22  drv_lcdc.o(i.drv_lcdc_config_edpi_mode)
    drv_lcdc_config_endianness               0x00016abf   Thumb Code    22  drv_lcdc.o(i.drv_lcdc_config_endianness)
    drv_lcdc_config_input_size               0x00016ad5   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_config_input_size)
    drv_lcdc_config_int                      0x00016ae1   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_config_int)
    drv_lcdc_config_int_single               0x00016aff   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_int_single)
    drv_lcdc_config_overwrite                0x00016b21   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_overwrite)
    drv_lcdc_config_overwrite_rgb            0x00016b43   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    drv_lcdc_config_partial_display_area     0x00016b4f   Thumb Code    26  drv_lcdc.o(i.drv_lcdc_config_partial_display_area)
    drv_lcdc_config_partial_display_enable   0x00016b69   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_partial_display_enable)
    drv_lcdc_config_scale_up_coef            0x00016b8b   Thumb Code    26  drv_lcdc.o(i.drv_lcdc_config_scale_up_coef)
    drv_lcdc_config_scale_up_step            0x00016ba5   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_config_scale_up_step)
    drv_lcdc_config_src_parameter            0x00016bb1   Thumb Code    76  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    drv_lcdc_config_thresh                   0x00016bfd   Thumb Code     6  drv_lcdc.o(i.drv_lcdc_config_thresh)
    drv_lcdc_ctrl_flow                       0x00016c03   Thumb Code    18  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    drv_lcdc_enable_shadow_reg               0x00016c15   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    drv_lcdc_set_int                         0x00016c35   Thumb Code    58  drv_lcdc.o(i.drv_lcdc_set_int)
    drv_lcdc_set_prefetch                    0x00016c75   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_set_prefetch)
    drv_lcdc_set_video_hw_mode               0x00016c8d   Thumb Code    20  drv_lcdc.o(i.drv_lcdc_set_video_hw_mode)
    drv_lcdc_start                           0x00016ca1   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_start)
    drv_memc_clear_status                    0x00016cc1   Thumb Code    12  drv_memc.o(i.drv_memc_clear_status)
    drv_memc_enable_irq                      0x00016ccd   Thumb Code    58  drv_memc.o(i.drv_memc_enable_irq)
    drv_memc_gen_a_tear_signal               0x00016d0d   Thumb Code    12  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    drv_memc_get_status                      0x00016d19   Thumb Code    18  drv_memc.o(i.drv_memc_get_status)
    drv_memc_rate_transfer_sel               0x00016d2b   Thumb Code    16  drv_memc.o(i.drv_memc_rate_transfer_sel)
    drv_memc_sel_vsync                       0x00016d3b   Thumb Code    14  drv_memc.o(i.drv_memc_sel_vsync)
    drv_memc_set_active_height               0x00016d49   Thumb Code    14  drv_memc.o(i.drv_memc_set_active_height)
    drv_memc_set_data_mode                   0x00016d5d   Thumb Code    12  drv_memc.o(i.drv_memc_set_data_mode)
    drv_memc_set_double_buffer               0x00016d69   Thumb Code    16  drv_memc.o(i.drv_memc_set_double_buffer)
    drv_memc_set_double_buffer_reverse       0x00016d79   Thumb Code    18  drv_memc.o(i.drv_memc_set_double_buffer_reverse)
    drv_memc_set_fs_en_conditions            0x00016d8b   Thumb Code    16  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    drv_memc_set_inten                       0x00016d9b   Thumb Code    20  drv_memc.o(i.drv_memc_set_inten)
    drv_memc_set_lcdc_st_conditions          0x00016db1   Thumb Code    18  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    drv_memc_set_ltpo_mode                   0x00016dc9   Thumb Code    26  drv_memc.o(i.drv_memc_set_ltpo_mode)
    drv_memc_set_tear_mode                   0x00016de3   Thumb Code    14  drv_memc.o(i.drv_memc_set_tear_mode)
    drv_memc_set_tear_waveform               0x00016df1   Thumb Code    34  drv_memc.o(i.drv_memc_set_tear_waveform)
    drv_memc_set_vidc_sync_cnt               0x00016e19   Thumb Code    14  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    drv_param_init_get_ccm                   0x00016e29   Thumb Code     4  drv_param_init.o(i.drv_param_init_get_ccm)
    drv_param_init_get_scld_filter_h         0x00016e31   Thumb Code    12  drv_param_init.o(i.drv_param_init_get_scld_filter_h)
    drv_param_init_get_scld_filter_v         0x00016e45   Thumb Code    12  drv_param_init.o(i.drv_param_init_get_scld_filter_v)
    drv_param_init_get_sclu_filter           0x00016e59   Thumb Code     4  drv_param_init.o(i.drv_param_init_get_sclu_filter)
    drv_param_init_set_ccm                   0x00016e61   Thumb Code    14  drv_param_init.o(i.drv_param_init_set_ccm)
    drv_param_p2r_filter_init                0x00016e75   Thumb Code    30  drv_param_init.o(i.drv_param_p2r_filter_init)
    drv_phy_enable_calibration               0x00016e99   Thumb Code    12  drv_phy_common.o(i.drv_phy_enable_calibration)
    drv_phy_get_calibration                  0x00016ea9   Thumb Code    50  drv_phy_common.o(i.drv_phy_get_calibration)
    drv_phy_get_pll_para                     0x00016ee5   Thumb Code    88  drv_phy_common.o(i.drv_phy_get_pll_para)
    drv_phy_get_rate_para                    0x00016f45   Thumb Code    76  drv_phy_common.o(i.drv_phy_get_rate_para)
    drv_phy_test_clear                       0x00016f99   Thumb Code    16  drv_phy_common.o(i.drv_phy_test_clear)
    drv_phy_test_lock                        0x00016fa9   Thumb Code    24  drv_phy_common.o(i.drv_phy_test_lock)
    drv_phy_test_write_1_byte                0x00016fc1   Thumb Code    32  drv_phy_common.o(i.drv_phy_test_write_1_byte)
    drv_phy_test_write_2_byte                0x00016fe1   Thumb Code    38  drv_phy_common.o(i.drv_phy_test_write_2_byte)
    drv_phy_test_write_code                  0x00017007   Thumb Code    30  drv_phy_common.o(i.drv_phy_test_write_code)
    drv_pwr_set_cp_mode                      0x00017045   Thumb Code    26  drv_pwr.o(i.drv_pwr_set_cp_mode)
    drv_pwr_set_pvd_mode                     0x00017065   Thumb Code    18  drv_pwr.o(i.drv_pwr_set_pvd_mode)
    drv_pwr_set_system_clk_src               0x0001707d   Thumb Code    44  drv_pwr.o(i.drv_pwr_set_system_clk_src)
    drv_rxbr_clear_pkt_buffer                0x000170fb   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    drv_rxbr_clear_status0                   0x00017105   Thumb Code     4  drv_rxbr.o(i.drv_rxbr_clear_status0)
    drv_rxbr_enable_irq                      0x00017109   Thumb Code    90  drv_rxbr.o(i.drv_rxbr_enable_irq)
    drv_rxbr_frame_drop_cfg                  0x00017165   Thumb Code    16  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    drv_rxbr_get_clk                         0x00017179   Thumb Code    66  drv_rxbr.o(i.drv_rxbr_get_clk)
    drv_rxbr_get_col_addr                    0x000171dd   Thumb Code     4  drv_rxbr.o(i.drv_rxbr_get_col_addr)
    drv_rxbr_get_page_addr                   0x000171f3   Thumb Code     4  drv_rxbr.o(i.drv_rxbr_get_page_addr)
    drv_rxbr_hline_rcv0_cfg                  0x00017209   Thumb Code    12  drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg)
    drv_rxbr_hline_rcv_cfg                   0x00017215   Thumb Code     8  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    drv_rxbr_register_irq0_callback          0x0001721d   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_register_irq0_callback)
    drv_rxbr_register_irq1_callback          0x00017229   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    drv_rxbr_set_ack_pkt_header              0x00017235   Thumb Code    20  drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header)
    drv_rxbr_set_cmd_filter                  0x00017249   Thumb Code   204  drv_rxbr.o(i.drv_rxbr_set_cmd_filter)
    drv_rxbr_set_color_format                0x00017315   Thumb Code    20  drv_rxbr.o(i.drv_rxbr_set_color_format)
    drv_rxbr_set_inten                       0x00017329   Thumb Code    20  drv_rxbr.o(i.drv_rxbr_set_inten)
    drv_rxbr_set_ltpo_drop_th                0x0001733d   Thumb Code    16  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    drv_rxbr_set_usr_cfg                     0x0001734d   Thumb Code    38  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    drv_rxbr_set_usr_col                     0x00017373   Thumb Code     8  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    drv_rxbr_set_usr_row                     0x0001737b   Thumb Code     8  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    drv_spi_m_read_data                      0x00017385   Thumb Code    28  drv_spi_master.o(i.drv_spi_m_read_data)
    drv_swire_set_int                        0x000173a5   Thumb Code    76  drv_swire.o(i.drv_swire_set_int)
    drv_swire_set_power_down                 0x000173f9   Thumb Code    24  drv_swire.o(i.drv_swire_set_power_down)
    drv_sys_cfg_clear_all_int                0x00017415   Thumb Code     8  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    drv_sys_cfg_clear_pending                0x00017421   Thumb Code    32  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    drv_sys_cfg_sel_ap_rst_lvl_trig          0x00017449   Thumb Code    18  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig)
    drv_sys_cfg_sel_ap_rst_trig              0x00017461   Thumb Code    22  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig)
    drv_sys_cfg_sel_gpio_group               0x0001747d   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group)
    drv_sys_cfg_sel_int_trig                 0x000174a1   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig)
    drv_sys_cfg_set_dma_rx_req               0x000174c5   Thumb Code    10  drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req)
    drv_sys_cfg_set_dma_tx_req               0x000174d5   Thumb Code    10  drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req)
    drv_sys_cfg_set_int                      0x000174e5   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    drv_timer_enable                         0x00017523   Thumb Code    32  drv_timer.o(i.drv_timer_enable)
    drv_timer_get_instance                   0x00017545   Thumb Code    10  drv_timer.o(i.drv_timer_get_instance)
    drv_timer_get_prescaler                  0x00017555   Thumb Code    12  drv_timer.o(i.drv_timer_get_prescaler)
    drv_timer_register_callback              0x000175a9   Thumb Code    14  drv_timer.o(i.drv_timer_register_callback)
    drv_timer_set_compare_val                0x000175bd   Thumb Code    16  drv_timer.o(i.drv_timer_set_compare_val)
    drv_timer_set_int                        0x000175cd   Thumb Code    80  drv_timer.o(i.drv_timer_set_int)
    drv_timer_set_prescaler                  0x00017621   Thumb Code    36  drv_timer.o(i.drv_timer_set_prescaler)
    drv_tx_phy_test_enter                    0x00017653   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    drv_tx_phy_test_exit                     0x0001766f   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    drv_vidc_clear_irq                       0x000176c1   Thumb Code     8  drv_vidc.o(i.drv_vidc_clear_irq)
    drv_vidc_enable                          0x000176c9   Thumb Code    24  drv_vidc.o(i.drv_vidc_enable)
    drv_vidc_enable_irq                      0x000176e1   Thumb Code    58  drv_vidc.o(i.drv_vidc_enable_irq)
    drv_vidc_get_irq_status                  0x00017721   Thumb Code    18  drv_vidc.o(i.drv_vidc_get_irq_status)
    drv_vidc_init_module_enable              0x00017735   Thumb Code    36  drv_vidc.o(i.drv_vidc_init_module_enable)
    drv_vidc_register_callback               0x0001775d   Thumb Code     6  drv_vidc.o(i.drv_vidc_register_callback)
    drv_vidc_reset                           0x00017769   Thumb Code     6  drv_vidc.o(i.drv_vidc_reset)
    drv_vidc_set_dst_parameter               0x0001776f   Thumb Code    60  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    drv_vidc_set_irqen                       0x000177ab   Thumb Code    20  drv_vidc.o(i.drv_vidc_set_irqen)
    drv_vidc_set_mirror                      0x000177bf   Thumb Code    16  drv_vidc.o(i.drv_vidc_set_mirror)
    drv_vidc_set_p2r_hcoef0                  0x000177cf   Thumb Code     8  drv_vidc.o(i.drv_vidc_set_p2r_hcoef0)
    drv_vidc_set_p2r_hinitb                  0x000177d7   Thumb Code    38  drv_vidc.o(i.drv_vidc_set_p2r_hinitb)
    drv_vidc_set_p2r_hinitr                  0x000177fd   Thumb Code    38  drv_vidc.o(i.drv_vidc_set_p2r_hinitr)
    drv_vidc_set_pentile_swap                0x00017825   Thumb Code    18  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    drv_vidc_set_pu_ctrl                     0x0001783d   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    drv_vidc_set_rotation                    0x00017847   Thumb Code    16  drv_vidc.o(i.drv_vidc_set_rotation)
    drv_vidc_set_scld_hcoef0                 0x00017857   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    drv_vidc_set_scld_hcoef1                 0x00017861   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    drv_vidc_set_scld_step                   0x0001786b   Thumb Code    18  drv_vidc.o(i.drv_vidc_set_scld_step)
    drv_vidc_set_scld_vcoef0                 0x0001787d   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    drv_vidc_set_scld_vcoef1                 0x00017887   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    drv_vidc_set_src_parameter               0x00017891   Thumb Code    22  drv_vidc.o(i.drv_vidc_set_src_parameter)
    drv_wdg_clear_counter                    0x000178a9   Thumb Code    12  drv_wdg.o(i.drv_wdg_clear_counter)
    drv_wdg_set_int                          0x000178d9   Thumb Code    60  drv_wdg.o(i.drv_wdg_set_int)
    fls_clr_interrupt_flag                   0x00017919   Thumb Code    10  drv_fls.o(i.fls_clr_interrupt_flag)
    fputc                                    0x00017923   Thumb Code    20  tau_log.o(i.fputc)
    hal_dsi_rx_ctrl_create_handle            0x00017939   Thumb Code    48  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    hal_dsi_rx_ctrl_deinit                   0x0001796d   Thumb Code   148  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit)
    hal_dsi_rx_ctrl_dsc_async_handler        0x00017a09   Thumb Code   120  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler)
    hal_dsi_rx_ctrl_gen_a_tear_signal        0x00017a8d   Thumb Code    32  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal)
    hal_dsi_rx_ctrl_get_max_ret_size         0x00017ab5   Thumb Code    30  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size)
    hal_dsi_rx_ctrl_hight_performan_mode     0x00017add   Thumb Code    16  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode)
    hal_dsi_rx_ctrl_init                     0x00017b41   Thumb Code   144  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    hal_dsi_rx_ctrl_pre_init_pps             0x00018321   Thumb Code    56  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    hal_dsi_rx_ctrl_send_ack_cmd             0x0001835d   Thumb Code   212  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd)
    hal_dsi_rx_ctrl_set_cus_sync_line        0x0001844d   Thumb Code    44  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line)
    hal_dsi_rx_ctrl_set_hw_tear_mode         0x00018481   Thumb Code    42  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode)
    hal_dsi_rx_ctrl_set_sw_tear_mode         0x00018561   Thumb Code    42  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode)
    hal_dsi_rx_ctrl_set_tear_mode_ex         0x00018595   Thumb Code    14  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex)
    hal_dsi_rx_ctrl_start                    0x000185a5   Thumb Code    46  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    hal_dsi_rx_ctrl_stop                     0x000185e1   Thumb Code    46  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop)
    hal_dsi_rx_ctrl_toggle_resolution        0x0001861d   Thumb Code    28  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    hal_dsi_tx_ctrl_create_handle            0x00018c51   Thumb Code    34  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    hal_dsi_tx_ctrl_deinit                   0x00018c7d   Thumb Code   118  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit)
    hal_dsi_tx_ctrl_enter_init_panel_mode    0x00018d01   Thumb Code    68  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode)
    hal_dsi_tx_ctrl_exit_init_panel_mode     0x00018d4d   Thumb Code    32  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode)
    hal_dsi_tx_ctrl_init                     0x00018d75   Thumb Code   154  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    hal_dsi_tx_ctrl_panel_reset_pin          0x00018e3d   Thumb Code    12  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin)
    hal_dsi_tx_ctrl_set_ccm                  0x00018e49   Thumb Code    28  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm)
    hal_dsi_tx_ctrl_set_overwrite_rgb        0x00018e69   Thumb Code    16  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    hal_dsi_tx_ctrl_set_partial_disp         0x00018e7d   Thumb Code    12  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp)
    hal_dsi_tx_ctrl_set_partial_disp_area    0x00018e8d   Thumb Code    30  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area)
    hal_dsi_tx_ctrl_start                    0x00018eb1   Thumb Code   140  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    hal_dsi_tx_ctrl_stop                     0x00018f4d   Thumb Code    56  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop)
    hal_dsi_tx_ctrl_write_array_cmd          0x00018f91   Thumb Code   210  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd)
    hal_dsi_tx_ctrl_write_cmd                0x00019069   Thumb Code   172  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    hal_gpio_ctrl_eint                       0x000192fd   Thumb Code    18  hal_gpio.o(i.hal_gpio_ctrl_eint)
    hal_gpio_get_input_data                  0x00019315   Thumb Code    18  hal_gpio.o(i.hal_gpio_get_input_data)
    hal_gpio_init_eint                       0x00019329   Thumb Code    58  hal_gpio.o(i.hal_gpio_init_eint)
    hal_gpio_init_input                      0x00019369   Thumb Code    28  hal_gpio.o(i.hal_gpio_init_input)
    hal_gpio_init_output                     0x00019389   Thumb Code    34  hal_gpio.o(i.hal_gpio_init_output)
    hal_gpio_reg_eint_cb                     0x000193b1   Thumb Code    20  hal_gpio.o(i.hal_gpio_reg_eint_cb)
    hal_gpio_set_ap_reset_int                0x000193c9   Thumb Code    76  hal_gpio.o(i.hal_gpio_set_ap_reset_int)
    hal_gpio_set_mode                        0x00019419   Thumb Code    90  hal_gpio.o(i.hal_gpio_set_mode)
    hal_gpio_set_output_data                 0x00019479   Thumb Code     8  hal_gpio.o(i.hal_gpio_set_output_data)
    hal_gpio_set_pull_state                  0x00019481   Thumb Code    26  hal_gpio.o(i.hal_gpio_set_pull_state)
    hal_i2c_m_dma_init                       0x000194a1   Thumb Code    92  hal_i2c_master.o(i.hal_i2c_m_dma_init)
    hal_i2c_m_dma_read                       0x0001950d   Thumb Code    26  hal_i2c_master.o(i.hal_i2c_m_dma_read)
    hal_i2c_m_dma_write                      0x0001952d   Thumb Code    24  hal_i2c_master.o(i.hal_i2c_m_dma_write)
    hal_i2c_m_transfer_complate              0x00019549   Thumb Code     6  hal_i2c_master.o(i.hal_i2c_m_transfer_complate)
    hal_i2c_s_dma_write                      0x00019585   Thumb Code    62  hal_i2c_slave.o(i.hal_i2c_s_dma_write)
    hal_i2c_s_init                           0x000195d1   Thumb Code   176  hal_i2c_slave.o(i.hal_i2c_s_init)
    hal_i2c_s_nonblocking_read               0x00019699   Thumb Code    14  hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read)
    hal_i2c_s_set_transfer                   0x000196ad   Thumb Code     6  hal_i2c_slave.o(i.hal_i2c_s_set_transfer)
    hal_internal_init_memc                   0x0001982d   Thumb Code   170  hal_internal_vsync.o(i.hal_internal_init_memc)
    hal_internal_sync_get_fb_setting         0x00019929   Thumb Code    12  hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting)
    hal_internal_sync_get_hight_performan_mode 0x00019939   Thumb Code    10  hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode)
    hal_internal_sync_input_resolution_change 0x00019949   Thumb Code   438  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    hal_internal_update_dpi_param            0x00019b75   Thumb Code    10  hal_internal_vsync.o(i.hal_internal_update_dpi_param)
    hal_internal_video_mode_auto_sync        0x00019b85   Thumb Code   270  hal_internal_vsync.o(i.hal_internal_video_mode_auto_sync)
    hal_internal_vsync_deinit                0x00019cb1   Thumb Code    30  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    hal_internal_vsync_get_rx_state          0x00019cd9   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state)
    hal_internal_vsync_get_sync_line         0x00019ce5   Thumb Code    18  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    hal_internal_vsync_get_tear_mode         0x00019cfd   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_tear_mode)
    hal_internal_vsync_get_tx_state          0x00019d09   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    hal_internal_vsync_init_rx               0x00019d15   Thumb Code   236  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    hal_internal_vsync_init_tx               0x00019e2d   Thumb Code   172  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    hal_internal_vsync_set_auto_hw_filter    0x00019edd   Thumb Code   222  hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter)
    hal_internal_vsync_set_rx_state          0x00019ff9   Thumb Code    16  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    hal_internal_vsync_set_sync_line         0x0001a00d   Thumb Code    30  hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line)
    hal_internal_vsync_set_tear_mode         0x0001a031   Thumb Code    72  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    hal_internal_vsync_set_tx_state          0x0001a081   Thumb Code   118  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    hal_spi_m_clear_rxfifo                   0x0001a539   Thumb Code    14  hal_spi_master.o(i.hal_spi_m_clear_rxfifo)
    hal_swire_open                           0x0001a547   Thumb Code    22  hal_swire.o(i.hal_swire_open)
    hal_system_enable_systick                0x0001a55d   Thumb Code     8  hal_system.o(i.hal_system_enable_systick)
    hal_system_init                          0x0001a565   Thumb Code   104  hal_system.o(i.hal_system_init)
    hal_system_init_console                  0x0001a5ed   Thumb Code    28  hal_system.o(i.hal_system_init_console)
    hal_system_set_phy_calibration           0x0001a609   Thumb Code     8  hal_system.o(i.hal_system_set_phy_calibration)
    hal_system_set_pvd                       0x0001a611   Thumb Code     8  hal_system.o(i.hal_system_set_pvd)
    hal_system_set_vcc                       0x0001a619   Thumb Code     8  hal_system.o(i.hal_system_set_vcc)
    hal_timer_init                           0x0001a621   Thumb Code    26  hal_timer.o(i.hal_timer_init)
    hal_timer_start                          0x0001a63d   Thumb Code    66  hal_timer.o(i.hal_timer_start)
    hal_timer_stop                           0x0001a685   Thumb Code    40  hal_timer.o(i.hal_timer_stop)
    hal_uart_init                            0x0001a6ad   Thumb Code   126  hal_uart.o(i.hal_uart_init)
    hal_uart_transmit_blocking               0x0001a739   Thumb Code    12  hal_uart.o(i.hal_uart_transmit_blocking)
    handle_init                              0x0001a749   Thumb Code   140  irq_redirect .o(i.handle_init)
    main                                     0x0001a945   Thumb Code    10  main.o(i.main)
    sqrt                                     0x0001b5f1   Thumb Code    66  sqrt.o(i.sqrt)
    tp_heartbeat_exec                        0x0001b639   Thumb Code    50  ap_demo.o(i.tp_heartbeat_exec)
    phone_data_21                            0x0001bc2c   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_55                            0x0001bc2d   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_85_1                          0x0001bc2e   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_92_1                          0x0001bc2f   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_F5_1                          0x0001bc30   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_F5_2                          0x0001bc31   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_F5_3                          0x0001bc32   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_F5_4                          0x0001bc33   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_30                            0x0001bc34   Data           2  app_tp_for_custom_s8.o(.constdata)
    phone_data_52                            0x0001bc36   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_data_92_3                          0x0001bc39   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_data_A3                            0x0001bc3c   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_data_A4                            0x0001bc40   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_data_A5                            0x0001bc44   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_data_AF                            0x0001bc48   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_data_F1                            0x0001bc4c   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_data_22                            0x0001bc50   Data           5  app_tp_for_custom_s8.o(.constdata)
    phone_data_92_2                          0x0001bc55   Data           6  app_tp_for_custom_s8.o(.constdata)
    phone_data_F6_1                          0x0001bc5b   Data           6  app_tp_for_custom_s8.o(.constdata)
    phone_data_F6_2                          0x0001bc61   Data           6  app_tp_for_custom_s8.o(.constdata)
    phone_data_F6_3                          0x0001bc67   Data           6  app_tp_for_custom_s8.o(.constdata)
    phone_data_F6_4                          0x0001bc6d   Data           6  app_tp_for_custom_s8.o(.constdata)
    phone_data_60_1                          0x0001bc73   Data          16  app_tp_for_custom_s8.o(.constdata)
    phone_data_23                            0x0001bc83   Data          11  app_tp_for_custom_s8.o(.constdata)
    phone_data_85_2                          0x0001bc8e   Data          28  app_tp_for_custom_s8.o(.constdata)
    phone_data_90                            0x0001bcaa   Data          10  app_tp_for_custom_s8.o(.constdata)
    phone_data_72_0                          0x0001bcb4   Data        1292  app_tp_for_custom_s8.o(.constdata)
    phone_data_72_5                          0x0001c1c0   Data        1292  app_tp_for_custom_s8.o(.constdata)
    phone_data_72_13                         0x0001c6cc   Data        1292  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_01                         0x0001cbd8   Data         654  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_02                         0x0001ce66   Data         654  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_03                         0x0001d0f4   Data         654  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_06                         0x0001d382   Data         654  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_07                         0x0001d610   Data         654  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_05                         0x0001d89e   Data         654  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_00                         0x0001db2c   Data         288  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_FF                         0x0001dc4c   Data         288  app_tp_for_custom_s8.o(.constdata)
    sleep_on                                 0x0001dd6c   Data          16  app_tp_for_custom_s8.o(.constdata)
    screen_reg_start_data_size               0x0001dd7c   Data           1  app_tp_for_custom_s8.o(.constdata)
    Region$$Table$$Base                      0x0001e0d0   Number         0  anon$$obj.o(Region$$Table)
    Region$$Table$$Limit                     0x0001e100   Number         0  anon$$obj.o(Region$$Table)
    g_fun_handle                             0x00070100   Data         192  irq_redirect .o(.ARM.__AT_0x00070100)
    phone_86_flag                            0x000701d7   Data           1  ap_demo.o(.data)
    phone_A6_flag                            0x000701d8   Data           1  ap_demo.o(.data)
    phone_start_flag                         0x000701d9   Data           1  ap_demo.o(.data)
    phone_DisplayOFF_flag                    0x000701da   Data           1  ap_demo.o(.data)
    ap_tear_flag                             0x000701dc   Data           1  ap_demo.o(.data)
    g_enter_display_off                      0x000701dd   Data           1  ap_demo.o(.data)
    g_enter_display_ON                       0x000701de   Data           1  ap_demo.o(.data)
    panel_mode                               0x000701e0   Data           1  ap_demo.o(.data)
    phone_DisplayOFF_count                   0x000701e8   Data           2  ap_demo.o(.data)
    value_reg_b1                             0x000701ea   Data           2  ap_demo.o(.data)
    value_reg_b1_bak                         0x000701ec   Data           2  ap_demo.o(.data)
    value_reg51                              0x000701ee   Data           2  ap_demo.o(.data)
    value_reg51_bak                          0x000701f0   Data           2  ap_demo.o(.data)
    panel_r                                  0x000701f2   Data           2  ap_demo.o(.data)
    panel_g                                  0x000701f4   Data           2  ap_demo.o(.data)
    panel_b                                  0x000701f6   Data           2  ap_demo.o(.data)
    s_heartbeat                              0x00070200   Data           4  ap_demo.o(.data)
    value_reg_ca                             0x00070204   Data           4  ap_demo.o(.data)
    panel_init_code                          0x0007020c   Data        7466  ap_demo.o(.data)
    s_screen_init_complate                   0x00071f3a   Data           1  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data1               0x00071f3e   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data3               0x00071f41   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data4               0x00071f44   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data2               0x00071f47   Data           6  app_tp_transfer.o(.data)
    st_touch_init_sensor_off                 0x00071f4f   Data           3  app_tp_st_touch.o(.data)
    st_touch_init_sensor_on                  0x00071f52   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_reset                 0x00071f55   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_FpnlInit              0x00071f58   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_PnlInit               0x00071f5b   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_SvCfg                 0x00071f5e   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_SvCx                  0x00071f61   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_SvPnl                 0x00071f64   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_clearfifo             0x00071f67   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_clkreset              0x00071f6a   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_TuneM                 0x00071f6d   Data           4  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_TuneS                 0x00071f71   Data           4  app_tp_st_touch.o(.data)
    phone_data_E4                            0x00071fa4   Data           1  app_tp_for_custom_s8.o(.data)
    tp_flag                                  0x00071fa5   Data           1  app_tp_for_custom_s8.o(.data)
    g_phone_output_int_pad                   0x00071fa6   Data           1  app_tp_for_custom_s8.o(.data)
    tp_sleep_in                              0x00071fa7   Data           1  app_tp_for_custom_s8.o(.data)
    tp_sleep_count                           0x00071fa8   Data           1  app_tp_for_custom_s8.o(.data)
    sleep_double_EN                          0x00071fa9   Data           1  app_tp_for_custom_s8.o(.data)
    Flag_EA_EN                               0x00071faa   Data           1  app_tp_for_custom_s8.o(.data)
    Flag_touch_count                         0x00071fab   Data           1  app_tp_for_custom_s8.o(.data)
    touchnum_bak                             0x00071fac   Data           1  app_tp_for_custom_s8.o(.data)
    Flag_blacklight_EN                       0x00071fad   Data           1  app_tp_for_custom_s8.o(.data)
    phone_data_B1                            0x00071fb6   Data           2  app_tp_for_custom_s8.o(.data)
    phone_reg_coord_back                     0x00071fc0   Data         200  app_tp_for_custom_s8.o(.data)
    g_screen_input_rst_pad                   0x00072088   Data           1  app_tp_for_custom_s8.o(.data)
    g_screen_input_int_pad                   0x00072089   Data           1  app_tp_for_custom_s8.o(.data)
    screen_data_write_1                      0x0007208a   Data           1  app_tp_for_custom_s8.o(.data)
    screen_data_write_2                      0x0007208b   Data           3  app_tp_for_custom_s8.o(.data)
    screen_data_write_3                      0x0007208e   Data           5  app_tp_for_custom_s8.o(.data)
    screen_reg_int_data                      0x00072094   Data          48  app_tp_for_custom_s8.o(.data)
    g_sof_gen_te_func                        0x000720cc   Data           4  hal_internal_vsync.o(.data)
    g_systick_cb_func                        0x000720e0   Data           4  drv_common.o(.data)
    g_system_clock                           0x000720e4   Data           4  drv_common.o(.data)
    g_scld_fhd_filter_h                      0x000720fc   Data         256  drv_param_init.o(.data)
    g_scld_fhd_filter_v                      0x000721fc   Data         256  drv_param_init.o(.data)
    g_scld_hd_filter_h                       0x000722fc   Data         256  drv_param_init.o(.data)
    g_scld_hd_filter_v                       0x000723fc   Data         256  drv_param_init.o(.data)
    g_sclu_lanczos_filter                    0x000724fc   Data         128  drv_param_init.o(.data)
    g_ccm_setting                            0x0007257c   Data          36  drv_param_init.o(.data)
    g_int_rxbr_irq0_cb_func                  0x00072600   Data           4  drv_rxbr.o(.data)
    g_int_rxbr_irq1_cb_func                  0x00072604   Data           4  drv_rxbr.o(.data)
    g_int_vidc_cb_func                       0x00072608   Data           4  drv_vidc.o(.data)
    g_fls_w_cmd                              0x00072624   Data           1  norflash.o(.data)
    g_fls_r_cmd                              0x00072625   Data           1  norflash.o(.data)
    g_fls_write_en_status                    0x00072626   Data           1  norflash.o(.data)
    isFlsTransferEnd                         0x00072627   Data           1  norflash.o(.data)
    isFlsFifoReq                             0x00072628   Data           1  norflash.o(.data)
    isNandWriteCompleted                     0x00072629   Data           1  norflash.o(.data)
    isNandReadCompleted                      0x0007262a   Data           1  norflash.o(.data)
    g_fls_error_info                         0x00072630   Data           6  norflash.o(.data)
    __stdout                                 0x00072658   Data           4  stdout.o(.data)
    tp_scan_data                             0x000727f0   Data          12  app_tp_st_touch.o(.bss)
    hal_dmahandle                            0x0007290c   Data         160  hal_uart.o(.bss)
    hal_uarthandle_dma                       0x000729ac   Data          32  hal_uart.o(.bss)
    hal_uart_handle_global                   0x000729cc   Data          16  hal_uart.o(.bss)
    g_vsync_hande                            0x000729dc   Data         100  hal_internal_vsync.o(.bss)
    g_dcs_execute_table                      0x00072a40   Data        2048  hal_internal_vsync.o(.bss)
    g_packet_fifo                            0x000734fc   Data        4144  dcs_packet_fifo.o(.bss)
    string                                   0x0007452c   Data         256  tau_log.o(.bss)
    g_spis_ctrl_handle                       0x0007462c   Data          32  hal_spi_slave.o(.bss)
    __stack_limit                            0x00074650   Data           0  startup_armcm0.o(STACK)
    __initial_sp                             0x00075650   Data           0  startup_armcm0.o(STACK)



==============================================================================

Memory Map of the image

  Image Entry point : 0x000100c1

  Load Region LR_IROM2 (Base: 0x00010000, Size: 0x00010590, Max: 0x00010000, ABSOLUTE, COMPRESSED[0x0000f550])

    Execution Region ER_IROM2 (Exec base: 0x00010000, Load base: 0x00010000, Size: 0x0000e100, Max: 0x00010000, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00010000   0x00010000   0x000000c0   Data   RO          538    RESET               startup_armcm0.o
    0x000100c0   0x000100c0   0x00000000   Code   RO         2779  * .ARM.Collect$$$$00000000  mc_p.l(entry.o)
    0x000100c0   0x000100c0   0x00000004   Code   RO         3089    .ARM.Collect$$$$00000001  mc_p.l(entry2.o)
    0x000100c4   0x000100c4   0x00000004   Code   RO         3092    .ARM.Collect$$$$00000004  mc_p.l(entry5.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         3094    .ARM.Collect$$$$00000008  mc_p.l(entry7b.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         3096    .ARM.Collect$$$$0000000A  mc_p.l(entry8b.o)
    0x000100c8   0x000100c8   0x00000008   Code   RO         3097    .ARM.Collect$$$$0000000B  mc_p.l(entry9a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         3099    .ARM.Collect$$$$0000000D  mc_p.l(entry10a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         3101    .ARM.Collect$$$$0000000F  mc_p.l(entry11a.o)
    0x000100d0   0x000100d0   0x00000004   Code   RO         3090    .ARM.Collect$$$$00002712  mc_p.l(entry2.o)
    0x000100d4   0x000100d4   0x00000078   Code   RO          539    .text               startup_armcm0.o
    0x0001014c   0x0001014c   0x0000002c   Code   RO         2782    .text               mc_p.l(uidiv.o)
    0x00010178   0x00010178   0x00000028   Code   RO         2784    .text               mc_p.l(idiv.o)
    0x000101a0   0x000101a0   0x00000024   Code   RO         2786    .text               mc_p.l(memcpya.o)
    0x000101c4   0x000101c4   0x00000024   Code   RO         2788    .text               mc_p.l(memseta.o)
    0x000101e8   0x000101e8   0x000000b2   Code   RO         3053    .text               mf_p.l(fadd.o)
    0x0001029a   0x0001029a   0x0000007a   Code   RO         3055    .text               mf_p.l(fmul.o)
    0x00010314   0x00010314   0x0000007c   Code   RO         3057    .text               mf_p.l(fdiv.o)
    0x00010390   0x00010390   0x00000018   Code   RO         3059    .text               mf_p.l(fscalb.o)
    0x000103a8   0x000103a8   0x00000164   Code   RO         3061    .text               mf_p.l(dadd.o)
    0x0001050c   0x0001050c   0x000000d0   Code   RO         3063    .text               mf_p.l(dmul.o)
    0x000105dc   0x000105dc   0x000000f0   Code   RO         3065    .text               mf_p.l(ddiv.o)
    0x000106cc   0x000106cc   0x00000016   Code   RO         3067    .text               mf_p.l(fflti.o)
    0x000106e2   0x000106e2   0x0000000e   Code   RO         3069    .text               mf_p.l(ffltui.o)
    0x000106f0   0x000106f0   0x0000001c   Code   RO         3073    .text               mf_p.l(dfltui.o)
    0x0001070c   0x0001070c   0x00000032   Code   RO         3075    .text               mf_p.l(ffixi.o)
    0x0001073e   0x0001073e   0x00000028   Code   RO         3077    .text               mf_p.l(ffixui.o)
    0x00010766   0x00010766   0x00000002   PAD
    0x00010768   0x00010768   0x00000048   Code   RO         3079    .text               mf_p.l(dfixi.o)
    0x000107b0   0x000107b0   0x0000003c   Code   RO         3081    .text               mf_p.l(dfixui.o)
    0x000107ec   0x000107ec   0x00000028   Code   RO         3083    .text               mf_p.l(f2d.o)
    0x00010814   0x00010814   0x00000028   Code   RO         3085    .text               mf_p.l(cdcmple.o)
    0x0001083c   0x0001083c   0x00000014   Code   RO         3087    .text               mf_p.l(cfrcmple.o)
    0x00010850   0x00010850   0x00000060   Code   RO         3104    .text               mc_p.l(uldiv.o)
    0x000108b0   0x000108b0   0x00000020   Code   RO         3106    .text               mc_p.l(llshl.o)
    0x000108d0   0x000108d0   0x00000022   Code   RO         3108    .text               mc_p.l(llushr.o)
    0x000108f2   0x000108f2   0x00000026   Code   RO         3110    .text               mc_p.l(llsshr.o)
    0x00010918   0x00010918   0x00000000   Code   RO         3119    .text               mc_p.l(iusefp.o)
    0x00010918   0x00010918   0x00000082   Code   RO         3120    .text               mf_p.l(fepilogue.o)
    0x0001099a   0x0001099a   0x000000be   Code   RO         3122    .text               mf_p.l(depilogue.o)
    0x00010a58   0x00010a58   0x000000a2   Code   RO         3126    .text               mf_p.l(dsqrt.o)
    0x00010afa   0x00010afa   0x00000002   PAD
    0x00010afc   0x00010afc   0x00000040   Code   RO         3128    .text               mf_p.l(dfixul.o)
    0x00010b3c   0x00010b3c   0x00000028   Code   RO         3130    .text               mf_p.l(cdrcmple.o)
    0x00010b64   0x00010b64   0x00000024   Code   RO         3132    .text               mc_p.l(init.o)
    0x00010b88   0x00010b88   0x00000056   Code   RO         3142    .text               mc_p.l(__dczerorl2.o)
    0x00010bde   0x00010bde   0x00000002   PAD
    0x00010be0   0x00010be0   0x00000018   Code   RO         2200    i.ADC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010bf8   0x00010bf8   0x00000018   Code   RO         2201    i.AP_NRESET_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c10   0x00010c10   0x00000014   Code   RO         2202    i.DMA_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c24   0x00010c24   0x0000001c   Code   RO         2203    i.EXTI_INT0_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c40   0x00010c40   0x0000001c   Code   RO         2204    i.EXTI_INT1_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c5c   0x00010c5c   0x0000001c   Code   RO         2205    i.EXTI_INT2_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c78   0x00010c78   0x0000001c   Code   RO         2206    i.EXTI_INT3_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c94   0x00010c94   0x0000001c   Code   RO         2207    i.EXTI_INT4_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010cb0   0x00010cb0   0x0000001c   Code   RO         2208    i.EXTI_INT5_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010ccc   0x00010ccc   0x0000001c   Code   RO         2209    i.EXTI_INT6_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010ce8   0x00010ce8   0x0000001c   Code   RO         2210    i.EXTI_INT7_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010d04   0x00010d04   0x00000064   Code   RO         2361    i.EncryptCheck      tp_EncryptCheck.lib(app_tp_enc.o)
    0x00010d68   0x00010d68   0x00000014   Code   RO         2211    i.FLSCTRL_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010d7c   0x00010d7c   0x00000074   Code   RO          102    i.Gpio_swire_output  ap_demo.o
    0x00010df0   0x00010df0   0x00000014   Code   RO         2212    i.HardFault_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e04   0x00010e04   0x00000018   Code   RO         2213    i.I2C0_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e1c   0x00010e1c   0x00000018   Code   RO         2214    i.I2C1_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e34   0x00010e34   0x00000018   Code   RO         2215    i.LCDC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e4c   0x00010e4c   0x00000028   Code   RO         2350    i.LOG_printf        CVWL568.lib(tau_log.o)
    0x00010e74   0x00010e74   0x00000018   Code   RO         2216    i.MEMC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e8c   0x00010e8c   0x00000018   Code   RO         2217    i.MIPI_RX_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010ea4   0x00010ea4   0x00000018   Code   RO         2218    i.MIPI_TX_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010ebc   0x00010ebc   0x0000001c   Code   RO         2219    i.PWMDET_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010ed8   0x00010ed8   0x0000001c   Code   RO         2220    i.SPIM_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010ef4   0x00010ef4   0x0000001c   Code   RO         2221    i.SPIS_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010f10   0x00010f10   0x0000001c   Code   RO         2222    i.SWIRE_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010f2c   0x00010f2c   0x00000018   Code   RO         2223    i.SysTick_Handler   CVWL568.lib(irq_redirect .o)
    0x00010f44   0x00010f44   0x00000018   Code   RO         2224    i.TIMER0_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010f5c   0x00010f5c   0x00000018   Code   RO         2225    i.TIMER1_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010f74   0x00010f74   0x00000018   Code   RO         2226    i.TIMER2_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010f8c   0x00010f8c   0x00000018   Code   RO         2227    i.TIMER3_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010fa4   0x00010fa4   0x0000001c   Code   RO         2657    i.UART0_IRQ_Handle  CVWL568.lib(drv_uart.o)
    0x00010fc0   0x00010fc0   0x00000002   Code   RO         2661    i.UART_DisableDma   CVWL568.lib(drv_uart.o)
    0x00010fc2   0x00010fc2   0x00000004   Code   RO         2667    i.UART_GetInstance  CVWL568.lib(drv_uart.o)
    0x00010fc6   0x00010fc6   0x00000002   PAD
    0x00010fc8   0x00010fc8   0x00000018   Code   RO         2228    i.UART_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010fe0   0x00010fe0   0x0000001a   Code   RO         2679    i.UART_SwitchSCLK   CVWL568.lib(drv_uart.o)
    0x00010ffa   0x00010ffa   0x00000002   Code   RO         3137    i.__scatterload_null  mc_p.l(handlers.o)
    0x00010ffc   0x00010ffc   0x00000004   Code   RO         1784    i.drv_dsi_rx_set_inten  CVWL568.lib(drv_dsi_rx.o)
    0x00011000   0x00011000   0x00000014   Data   RO         1196    .ARM.__at_0x11000   CVWL568.lib(drv_common.o)
    0x00011014   0x00011014   0x00000004   Code   RO         1830    i.drv_dsi_tx_command_put_payload  CVWL568.lib(drv_dsi_tx.o)
    0x00011018   0x00011018   0x00000004   Data   RO         1197    .ARM.__at_0x11018   CVWL568.lib(drv_common.o)
    0x0001101c   0x0001101c   0x00000144   Code   RO          274    i.S20_Start_init    app_tp_transfer.o
    0x00011160   0x00011160   0x00000024   Code   RO         2675    i.UART_ResetRxFIFO  CVWL568.lib(drv_uart.o)
    0x00011184   0x00011184   0x00000048   Code   RO         2678    i.UART_SetBaudRate  CVWL568.lib(drv_uart.o)
    0x000111cc   0x000111cc   0x00000134   Code   RO         2681    i.UART_TransferHandleIRQ  CVWL568.lib(drv_uart.o)
    0x00011300   0x00011300   0x0000001a   Code   RO         2683    i.UART_WriteBlocking  CVWL568.lib(drv_uart.o)
    0x0001131a   0x0001131a   0x00000002   PAD
    0x0001131c   0x0001131c   0x000000bc   Code   RO         2684    i.UART_init         CVWL568.lib(drv_uart.o)
    0x000113d8   0x000113d8   0x00000018   Code   RO         2229    i.VIDC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x000113f0   0x000113f0   0x00000018   Code   RO         2230    i.VPRE_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00011408   0x00011408   0x00000018   Code   RO         2231    i.WDG_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00011420   0x00011420   0x00000020   Code   RO         3025    i.__0printf         mc_p.l(printfa.o)
    0x00011440   0x00011440   0x00000024   Code   RO         3031    i.__0vsprintf       mc_p.l(printfa.o)
    0x00011464   0x00011464   0x0000002e   Code   RO         3124    i.__ARM_clz         mf_p.l(depilogue.o)
    0x00011492   0x00011492   0x0000001a   Code   RO          226    i.__ARM_common_switch8  ap_demo.o
    0x000114ac   0x000114ac   0x00000018   Code   RO         1517    i.__NVIC_ClearPendingIRQ  CVWL568.lib(drv_i2c_master.o)
    0x000114c4   0x000114c4   0x00000018   Code   RO         1641    i.__NVIC_ClearPendingIRQ  CVWL568.lib(drv_spi_master.o)
    0x000114dc   0x000114dc   0x00000020   Code   RO         2054    i.__NVIC_DisableIRQ  CVWL568.lib(drv_rxbr.o)
    0x000114fc   0x000114fc   0x00000018   Code   RO         2055    i.__NVIC_EnableIRQ  CVWL568.lib(drv_rxbr.o)
    0x00011514   0x00011514   0x00000044   Code   RO         2438    i.__NVIC_SetPriority  CVWL568.lib(hal_spi_slave.o)
    0x00011558   0x00011558   0x0000000e   Code   RO         3136    i.__scatterload_copy  mc_p.l(handlers.o)
    0x00011566   0x00011566   0x0000000e   Code   RO         3138    i.__scatterload_zeroinit  mc_p.l(handlers.o)
    0x00011574   0x00011574   0x0000000c   Code   RO         3114    i.__set_errno       mc_p.l(errno.o)
    0x00011580   0x00011580   0x00000174   Code   RO         3032    i._fp_digits        mc_p.l(printfa.o)
    0x000116f4   0x000116f4   0x000006ec   Code   RO         3033    i._printf_core      mc_p.l(printfa.o)
    0x00011de0   0x00011de0   0x00000020   Code   RO         3034    i._printf_post_padding  mc_p.l(printfa.o)
    0x00011e00   0x00011e00   0x0000002c   Code   RO         3035    i._printf_pre_padding  mc_p.l(printfa.o)
    0x00011e2c   0x00011e2c   0x0000000a   Code   RO         3037    i._sputc            mc_p.l(printfa.o)
    0x00011e36   0x00011e36   0x00000002   PAD
    0x00011e38   0x00011e38   0x0000105c   Code   RO          103    i.ap_dcs_read       ap_demo.o
    0x00012e94   0x00012e94   0x00000138   Code   RO          104    i.ap_demo           ap_demo.o
    0x00012fcc   0x00012fcc   0x00000028   Code   RO          105    i.ap_get_reg_ca     ap_demo.o
    0x00012ff4   0x00012ff4   0x000000b0   Code   RO          106    i.ap_get_reg_df     ap_demo.o
    0x000130a4   0x000130a4   0x00000020   Code   RO          416    i.ap_get_tp_calibration_status_01  app_tp_st_touch.o
    0x000130c4   0x000130c4   0x00000028   Code   RO          107    i.ap_reset_cb       ap_demo.o
    0x000130ec   0x000130ec   0x000002c0   Code   RO          108    i.ap_set_backlight  ap_demo.o
    0x000133ac   0x000133ac   0x00000024   Code   RO          109    i.ap_set_display_off  ap_demo.o
    0x000133d0   0x000133d0   0x0000000c   Code   RO          110    i.ap_set_display_on  ap_demo.o
    0x000133dc   0x000133dc   0x00000038   Code   RO          111    i.ap_set_enter_sleep_mode  ap_demo.o
    0x00013414   0x00013414   0x0000000c   Code   RO          112    i.ap_set_exit_sleep_mode  ap_demo.o
    0x00013420   0x00013420   0x0000001c   Code   RO          113    i.ap_set_tp_calibration_04  ap_demo.o
    0x0001343c   0x0001343c   0x000000b0   Code   RO          418    i.ap_tp_st_touch_calibration  app_tp_st_touch.o
    0x000134ec   0x000134ec   0x0000001a   Code   RO          419    i.ap_tp_st_touch_error_handler_F3  app_tp_st_touch.o
    0x00013506   0x00013506   0x00000020   Code   RO          420    i.ap_tp_st_touch_error_handler_FF  app_tp_st_touch.o
    0x00013526   0x00013526   0x00000002   PAD
    0x00013528   0x00013528   0x000000a8   Code   RO          421    i.ap_tp_st_touch_get_calibration_success_mark  app_tp_st_touch.o
    0x000135d0   0x000135d0   0x0000001c   Code   RO          423    i.ap_tp_st_touch_scan_point_init  app_tp_st_touch.o
    0x000135ec   0x000135ec   0x00000094   Code   RO          424    i.ap_tp_st_touch_scan_point_record_event  app_tp_st_touch.o
    0x00013680   0x00013680   0x00000034   Code   RO          425    i.ap_tp_st_touch_scan_point_record_event_exec  app_tp_st_touch.o
    0x000136b4   0x000136b4   0x00000034   Code   RO          426    i.ap_tp_st_touch_simulate_finger_release_event  app_tp_st_touch.o
    0x000136e8   0x000136e8   0x00000070   Code   RO          427    i.ap_tp_st_touch_software_reset  app_tp_st_touch.o
    0x00013758   0x00013758   0x0000002c   Code   RO          114    i.ap_update_frame_rate  ap_demo.o
    0x00013784   0x00013784   0x0000001c   Code   RO         2056    i.app_ADC_IRQn_Handler  CVWL568.lib(drv_rxbr.o)
    0x000137a0   0x000137a0   0x00000024   Code   RO         1441    i.app_AP_NRESET_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x000137c4   0x000137c4   0x0000001c   Code   RO         1442    i.app_EXTI_INT0_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x000137e0   0x000137e0   0x0000001c   Code   RO         1443    i.app_EXTI_INT1_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x000137fc   0x000137fc   0x0000001c   Code   RO         1444    i.app_EXTI_INT2_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00013818   0x00013818   0x0000001c   Code   RO         1445    i.app_EXTI_INT3_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00013834   0x00013834   0x0000001c   Code   RO         1446    i.app_EXTI_INT4_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00013850   0x00013850   0x0000001c   Code   RO         1447    i.app_EXTI_INT5_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x0001386c   0x0001386c   0x0000001c   Code   RO         1448    i.app_EXTI_INT6_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00013888   0x00013888   0x0000001c   Code   RO         1449    i.app_EXTI_INT7_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x000138a4   0x000138a4   0x00000048   Code   RO         1188    i.app_HardFault_Handler  CVWL568.lib(drv_common.o)
    0x000138ec   0x000138ec   0x00000018   Code   RO         1552    i.app_I2C0_IRQn_Handler  CVWL568.lib(drv_i2c_slave.o)
    0x00013904   0x00013904   0x00000010   Code   RO         1518    i.app_I2C1_IRQn_Handler  CVWL568.lib(drv_i2c_master.o)
    0x00013914   0x00013914   0x000001a4   Code   RO         1093    i.app_LCDC_IRQn_Handler  CVWL568.lib(hal_internal_vsync.o)
    0x00013ab8   0x00013ab8   0x00000088   Code   RO         1998    i.app_MEMC_IRQn_Handler  CVWL568.lib(drv_memc.o)
    0x00013b40   0x00013b40   0x00000298   Code   RO         1770    i.app_MIPI_RX_IRQn_Handler  CVWL568.lib(drv_dsi_rx.o)
    0x00013dd8   0x00013dd8   0x000000a0   Code   RO         1826    i.app_MIPI_TX_IRQn_Handler  CVWL568.lib(drv_dsi_tx.o)
    0x00013e78   0x00013e78   0x00000048   Code   RO         2592    i.app_PWMDET_IRQn_Handler  CVWL568.lib(drv_pwm.o)
    0x00013ec0   0x00013ec0   0x00000030   Code   RO         1642    i.app_SPIM_IRQn_Handler  CVWL568.lib(drv_spi_master.o)
    0x00013ef0   0x00013ef0   0x00000200   Code   RO         2439    i.app_SPIS_IRQn_Handler  CVWL568.lib(hal_spi_slave.o)
    0x000140f0   0x000140f0   0x00000020   Code   RO         1674    i.app_SWIRE_IRQn_Handler  CVWL568.lib(drv_swire.o)
    0x00014110   0x00014110   0x00000018   Code   RO         1189    i.app_SysTick_Handler  CVWL568.lib(drv_common.o)
    0x00014128   0x00014128   0x0000000a   Code   RO         1724    i.app_TIMER0_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x00014132   0x00014132   0x0000000a   Code   RO         1725    i.app_TIMER1_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x0001413c   0x0001413c   0x0000000a   Code   RO         1726    i.app_TIMER2_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x00014146   0x00014146   0x0000000a   Code   RO         1727    i.app_TIMER3_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x00014150   0x00014150   0x00000008   Code   RO         2685    i.app_UART_IRQn_Handler  CVWL568.lib(drv_uart.o)
    0x00014158   0x00014158   0x0000001c   Code   RO         2121    i.app_VIDC_IRQn_Handler  CVWL568.lib(drv_vidc.o)
    0x00014174   0x00014174   0x0000001c   Code   RO         2057    i.app_VPRE_IRQn_Handler  CVWL568.lib(drv_rxbr.o)
    0x00014190   0x00014190   0x00000038   Code   RO         2744    i.app_WDG_IRQn_Handler  CVWL568.lib(drv_wdg.o)
    0x000141c8   0x000141c8   0x00000010   Code   RO         1303    i.app_dma_irq_handler  CVWL568.lib(drv_dma.o)
    0x000141d8   0x000141d8   0x00000030   Code   RO         2481    i.app_fls_ctrl_Handler  CVWL568.lib(norflash.o)
    0x00014208   0x00014208   0x00000024   Code   RO          275    i.app_tp_I2C_init   app_tp_transfer.o
    0x0001422c   0x0001422c   0x00000038   Code   RO          428    i.app_tp_calibration_exec  app_tp_st_touch.o
    0x00014264   0x00014264   0x00000030   Code   RO          276    i.app_tp_i2cs_callback  app_tp_transfer.o
    0x00014294   0x00014294   0x00000044   Code   RO          277    i.app_tp_init       app_tp_transfer.o
    0x000142d8   0x000142d8   0x00000020   Code   RO          278    i.app_tp_m_read     app_tp_transfer.o
    0x000142f8   0x000142f8   0x00000008   Code   RO          280    i.app_tp_m_write    app_tp_transfer.o
    0x00014300   0x00014300   0x0000041c   Code   RO          943    i.app_tp_phone_analysis_data  WL568_20U_HX667_TP.lib(app_tp_for_custom_s8.o)
    0x0001471c   0x0001471c   0x0000000c   Code   RO          281    i.app_tp_phone_clear_reset_on  app_tp_transfer.o
    0x00014728   0x00014728   0x00000008   Code   RO          283    i.app_tp_s_read     app_tp_transfer.o
    0x00014730   0x00014730   0x00000008   Code   RO          285    i.app_tp_s_write    app_tp_transfer.o
    0x00014738   0x00014738   0x000002dc   Code   RO          945    i.app_tp_screen_analysis_int  WL568_20U_HX667_TP.lib(app_tp_for_custom_s8.o)
    0x00014a14   0x00014a14   0x00000030   Code   RO          286    i.app_tp_screen_init  app_tp_transfer.o
    0x00014a44   0x00014a44   0x0000000c   Code   RO          287    i.app_tp_screen_int_callback  app_tp_transfer.o
    0x00014a50   0x00014a50   0x00000040   Code   RO          288    i.app_tp_transfer_screen_const  app_tp_transfer.o
    0x00014a90   0x00014a90   0x00000160   Code   RO          289    i.app_tp_transfer_screen_int  app_tp_transfer.o
    0x00014bf0   0x00014bf0   0x00000018   Code   RO          290    i.app_tp_transfer_screen_start  app_tp_transfer.o
    0x00014c08   0x00014c08   0x00000036   Code   RO          115    i.blue_change_ccm   ap_demo.o
    0x00014c3e   0x00014c3e   0x00000002   PAD
    0x00014c40   0x00014c40   0x00000024   Code   RO          518    i.board_Init        board.o
    0x00014c64   0x00014c64   0x000004f0   Code   RO         1094    i.calc_framebuffer_setting  CVWL568.lib(hal_internal_vsync.o)
    0x00015154   0x00015154   0x000000c8   Code   RO         2768    i.ceil              m_ps.l(ceil.o)
    0x0001521c   0x0001521c   0x0000002c   Code   RO         1095    i.check_mipi_rx_tx_video_info  CVWL568.lib(hal_internal_vsync.o)
    0x00015248   0x00015248   0x00000090   Code   RO         1096    i.check_pkt_buf_rev  CVWL568.lib(hal_internal_vsync.o)
    0x000152d8   0x000152d8   0x00000058   Code   RO         1757    i.dcs_packet_fifo_alloc  CVWL568.lib(dcs_packet_fifo.o)
    0x00015330   0x00015330   0x00000018   Code   RO         1758    i.dcs_packet_fifo_init  CVWL568.lib(dcs_packet_fifo.o)
    0x00015348   0x00015348   0x00000044   Code   RO         1759    i.dcs_packet_free_fifo_header  CVWL568.lib(dcs_packet_fifo.o)
    0x0001538c   0x0001538c   0x00000024   Code   RO         1760    i.dcs_packet_get_fifo_header  CVWL568.lib(dcs_packet_fifo.o)
    0x000153b0   0x000153b0   0x0000002c   Code   RO         1097    i.dcs_sw_filter     CVWL568.lib(hal_internal_vsync.o)
    0x000153dc   0x000153dc   0x00000018   Code   RO          935    i.delayMs           CVWL568.lib(tau_delay.o)
    0x000153f4   0x000153f4   0x00000022   Code   RO          936    i.delayUs           CVWL568.lib(tau_delay.o)
    0x00015416   0x00015416   0x00000002   PAD
    0x00015418   0x00015418   0x00000058   Code   RO          116    i.disable_mipi_timer_cb  ap_demo.o
    0x00015470   0x00015470   0x00000038   Code   RO         1693    i.drv_ap_rst_trig_edge_detect  CVWL568.lib(drv_sys_cfg.o)
    0x000154a8   0x000154a8   0x0000000c   Code   RO         2321    i.drv_chip_info_get_info  CVWL568.lib(drv_chip_info.o)
    0x000154b4   0x000154b4   0x00000040   Code   RO         2322    i.drv_chip_info_init  CVWL568.lib(drv_chip_info.o)
    0x000154f4   0x000154f4   0x000000b0   Code   RO         2323    i.drv_chip_rx_info_check  CVWL568.lib(drv_chip_info.o)
    0x000155a4   0x000155a4   0x00000014   Code   RO         2324    i.drv_chip_rx_init_done  CVWL568.lib(drv_chip_info.o)
    0x000155b8   0x000155b8   0x00000058   Code   RO         1191    i.drv_common_enable_systick  CVWL568.lib(drv_common.o)
    0x00015610   0x00015610   0x00000008   Code   RO         1194    i.drv_common_system_init  CVWL568.lib(drv_common.o)
    0x00015618   0x00015618   0x00000010   Code   RO         1216    i.drv_crgu_config_reset_modules  CVWL568.lib(drv_crgu.o)
    0x00015628   0x00015628   0x00000014   Code   RO         1229    i.drv_crgu_set_ahb_pre_div  CVWL568.lib(drv_crgu.o)
    0x0001563c   0x0001563c   0x00000014   Code   RO         1230    i.drv_crgu_set_ahb_src  CVWL568.lib(drv_crgu.o)
    0x00015650   0x00015650   0x00000020   Code   RO         1233    i.drv_crgu_set_clock  CVWL568.lib(drv_crgu.o)
    0x00015670   0x00015670   0x00000014   Code   RO         1234    i.drv_crgu_set_dpi_mux_src  CVWL568.lib(drv_crgu.o)
    0x00015684   0x00015684   0x00000018   Code   RO         1235    i.drv_crgu_set_dpi_pre_div  CVWL568.lib(drv_crgu.o)
    0x0001569c   0x0001569c   0x00000014   Code   RO         1236    i.drv_crgu_set_dpi_pre_src  CVWL568.lib(drv_crgu.o)
    0x000156b0   0x000156b0   0x00000014   Code   RO         1237    i.drv_crgu_set_dsc_core_div  CVWL568.lib(drv_crgu.o)
    0x000156c4   0x000156c4   0x00000014   Code   RO         1238    i.drv_crgu_set_dsco_src  CVWL568.lib(drv_crgu.o)
    0x000156d8   0x000156d8   0x00000014   Code   RO         1239    i.drv_crgu_set_dsco_src_div  CVWL568.lib(drv_crgu.o)
    0x000156ec   0x000156ec   0x00000014   Code   RO         1240    i.drv_crgu_set_fb_div  CVWL568.lib(drv_crgu.o)
    0x00015700   0x00015700   0x00000014   Code   RO         1241    i.drv_crgu_set_fb_src  CVWL568.lib(drv_crgu.o)
    0x00015714   0x00015714   0x00000014   Code   RO         1244    i.drv_crgu_set_lcdc_div  CVWL568.lib(drv_crgu.o)
    0x00015728   0x00015728   0x00000014   Code   RO         1245    i.drv_crgu_set_lcdc_src  CVWL568.lib(drv_crgu.o)
    0x0001573c   0x0001573c   0x00000014   Code   RO         1246    i.drv_crgu_set_mipi_cfg_src  CVWL568.lib(drv_crgu.o)
    0x00015750   0x00015750   0x00000018   Code   RO         1247    i.drv_crgu_set_mipi_ref_src  CVWL568.lib(drv_crgu.o)
    0x00015768   0x00015768   0x00000018   Code   RO         1250    i.drv_crgu_set_reset  CVWL568.lib(drv_crgu.o)
    0x00015780   0x00015780   0x00000014   Code   RO         1251    i.drv_crgu_set_rxbr_div  CVWL568.lib(drv_crgu.o)
    0x00015794   0x00015794   0x00000014   Code   RO         1252    i.drv_crgu_set_rxbr_src  CVWL568.lib(drv_crgu.o)
    0x000157a8   0x000157a8   0x00000014   Code   RO         1254    i.drv_crgu_set_vidc_src  CVWL568.lib(drv_crgu.o)
    0x000157bc   0x000157bc   0x00000018   Code   RO         1307    i.drv_dma_clear_flag  CVWL568.lib(drv_dma.o)
    0x000157d4   0x000157d4   0x0000001c   Code   RO         1308    i.drv_dma_create_handle  CVWL568.lib(drv_dma.o)
    0x000157f0   0x000157f0   0x00000010   Code   RO         1310    i.drv_dma_disenable_channel  CVWL568.lib(drv_dma.o)
    0x00015800   0x00015800   0x00000010   Code   RO         1312    i.drv_dma_enable_channel  CVWL568.lib(drv_dma.o)
    0x00015810   0x00015810   0x00000024   Code   RO         1313    i.drv_dma_enable_channel_interrupts  CVWL568.lib(drv_dma.o)
    0x00015834   0x00015834   0x0000000c   Code   RO         1315    i.drv_dma_get_channel_flag  CVWL568.lib(drv_dma.o)
    0x00015840   0x00015840   0x00000090   Code   RO         1318    i.drv_dma_irq_handler  CVWL568.lib(drv_dma.o)
    0x000158d0   0x000158d0   0x00000012   Code   RO         1320    i.drv_dma_prepar_transfer  CVWL568.lib(drv_dma.o)
    0x000158e2   0x000158e2   0x0000001a   Code   RO         1322    i.drv_dma_set_burst  CVWL568.lib(drv_dma.o)
    0x000158fc   0x000158fc   0x00000006   Code   RO         1323    i.drv_dma_set_callback  CVWL568.lib(drv_dma.o)
    0x00015902   0x00015902   0x00000002   PAD
    0x00015904   0x00015904   0x00000044   Code   RO         1325    i.drv_dma_set_transfer  CVWL568.lib(drv_dma.o)
    0x00015948   0x00015948   0x00000036   Code   RO         2334    i.drv_dsc_dec_convert_pps_rc_parameter  CVWL568.lib(drv_dsc_dec.o)
    0x0001597e   0x0001597e   0x0000000c   Code   RO         2335    i.drv_dsc_dec_disable  CVWL568.lib(drv_dsc_dec.o)
    0x0001598a   0x0001598a   0x00000002   PAD
    0x0001598c   0x0001598c   0x00000074   Code   RO         2336    i.drv_dsc_dec_enable  CVWL568.lib(drv_dsc_dec.o)
    0x00015a00   0x00015a00   0x0000000a   Code   RO         2337    i.drv_dsc_dec_get_nslc  CVWL568.lib(drv_dsc_dec.o)
    0x00015a0a   0x00015a0a   0x00000028   Code   RO         2339    i.drv_dsc_dec_set_u8_pps  CVWL568.lib(drv_dsc_dec.o)
    0x00015a32   0x00015a32   0x00000002   PAD
    0x00015a34   0x00015a34   0x00000104   Code   RO         1771    i.drv_dsi_rx_calc_ipi_tx_delay  CVWL568.lib(drv_dsi_rx.o)
    0x00015b38   0x00015b38   0x00000040   Code   RO         1772    i.drv_dsi_rx_enable_irq  CVWL568.lib(drv_dsi_rx.o)
    0x00015b78   0x00015b78   0x00000050   Code   RO         1773    i.drv_dsi_rx_get_color_bpp  CVWL568.lib(drv_dsi_rx.o)
    0x00015bc8   0x00015bc8   0x0000001c   Code   RO         1774    i.drv_dsi_rx_get_color_pcc  CVWL568.lib(drv_dsi_rx.o)
    0x00015be4   0x00015be4   0x00000008   Code   RO         1775    i.drv_dsi_rx_get_compression_en  CVWL568.lib(drv_dsi_rx.o)
    0x00015bec   0x00015bec   0x00000006   Code   RO         1776    i.drv_dsi_rx_get_max_ret_size  CVWL568.lib(drv_dsi_rx.o)
    0x00015bf2   0x00015bf2   0x0000000e   Code   RO         1780    i.drv_dsi_rx_power_up  CVWL568.lib(drv_dsi_rx.o)
    0x00015c00   0x00015c00   0x00000020   Code   RO         1781    i.drv_dsi_rx_set_ctrl_cfg  CVWL568.lib(drv_dsi_rx.o)
    0x00015c20   0x00015c20   0x00000010   Code   RO         1782    i.drv_dsi_rx_set_ddi_cfg  CVWL568.lib(drv_dsi_rx.o)
    0x00015c30   0x00015c30   0x00000010   Code   RO         1785    i.drv_dsi_rx_set_ipi_cfg  CVWL568.lib(drv_dsi_rx.o)
    0x00015c40   0x00015c40   0x00000046   Code   RO         1787    i.drv_dsi_rx_set_lane_swap  CVWL568.lib(drv_dsi_rx.o)
    0x00015c86   0x00015c86   0x00000026   Code   RO         1788    i.drv_dsi_rx_set_resp_cnt  CVWL568.lib(drv_dsi_rx.o)
    0x00015cac   0x00015cac   0x00000104   Code   RO         1789    i.drv_dsi_rx_set_up_phy  CVWL568.lib(drv_dsi_rx.o)
    0x00015db0   0x00015db0   0x0000000e   Code   RO         1790    i.drv_dsi_rx_shut_down  CVWL568.lib(drv_dsi_rx.o)
    0x00015dbe   0x00015dbe   0x00000014   Code   RO         1828    i.drv_dsi_tx_command_header  CVWL568.lib(drv_dsi_tx.o)
    0x00015dd2   0x00015dd2   0x0000006c   Code   RO         1829    i.drv_dsi_tx_command_mode_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x00015e3e   0x00015e3e   0x00000018   Code   RO         1831    i.drv_dsi_tx_config_eotp  CVWL568.lib(drv_dsi_tx.o)
    0x00015e56   0x00015e56   0x00000008   Code   RO         1832    i.drv_dsi_tx_config_int  CVWL568.lib(drv_dsi_tx.o)
    0x00015e5e   0x00015e5e   0x00000008   Code   RO         1833    i.drv_dsi_tx_dpi_lpcmd_time  CVWL568.lib(drv_dsi_tx.o)
    0x00015e66   0x00015e66   0x0000000a   Code   RO         1834    i.drv_dsi_tx_dpi_mode  CVWL568.lib(drv_dsi_tx.o)
    0x00015e70   0x00015e70   0x00000024   Code   RO         1835    i.drv_dsi_tx_dpi_polarity  CVWL568.lib(drv_dsi_tx.o)
    0x00015e94   0x00015e94   0x00000004   Code   RO         1836    i.drv_dsi_tx_edpi_cmd_size  CVWL568.lib(drv_dsi_tx.o)
    0x00015e98   0x00015e98   0x00000004   Code   RO         1838    i.drv_dsi_tx_get_cmd_status  CVWL568.lib(drv_dsi_tx.o)
    0x00015e9c   0x00015e9c   0x00000004   Code   RO         1840    i.drv_dsi_tx_mode   CVWL568.lib(drv_dsi_tx.o)
    0x00015ea0   0x00015ea0   0x00000018   Code   RO         1841    i.drv_dsi_tx_phy_clock_lane_auto_lp  CVWL568.lib(drv_dsi_tx.o)
    0x00015eb8   0x00015eb8   0x0000001a   Code   RO         1842    i.drv_dsi_tx_phy_clock_lane_req_hs  CVWL568.lib(drv_dsi_tx.o)
    0x00015ed2   0x00015ed2   0x0000000c   Code   RO         1844    i.drv_dsi_tx_phy_lane_mode  CVWL568.lib(drv_dsi_tx.o)
    0x00015ede   0x00015ede   0x00000064   Code   RO         1848    i.drv_dsi_tx_phy_status_ready  CVWL568.lib(drv_dsi_tx.o)
    0x00015f42   0x00015f42   0x0000003e   Code   RO         1849    i.drv_dsi_tx_phy_status_stopstate  CVWL568.lib(drv_dsi_tx.o)
    0x00015f80   0x00015f80   0x00000134   Code   RO         1851    i.drv_dsi_tx_phy_test_setup  CVWL568.lib(drv_dsi_tx.o)
    0x000160b4   0x000160b4   0x0000001e   Code   RO         1852    i.drv_dsi_tx_phy_time_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x000160d2   0x000160d2   0x00000008   Code   RO         1856    i.drv_dsi_tx_powerup  CVWL568.lib(drv_dsi_tx.o)
    0x000160da   0x000160da   0x0000001c   Code   RO         1857    i.drv_dsi_tx_response_mode  CVWL568.lib(drv_dsi_tx.o)
    0x000160f6   0x000160f6   0x00000018   Code   RO         1860    i.drv_dsi_tx_set_bta_ack  CVWL568.lib(drv_dsi_tx.o)
    0x0001610e   0x0001610e   0x0000000c   Code   RO         1861    i.drv_dsi_tx_set_esc_div  CVWL568.lib(drv_dsi_tx.o)
    0x0001611a   0x0001611a   0x00000002   PAD
    0x0001611c   0x0001611c   0x00000040   Code   RO         1862    i.drv_dsi_tx_set_int  CVWL568.lib(drv_dsi_tx.o)
    0x0001615c   0x0001615c   0x00000010   Code   RO         1863    i.drv_dsi_tx_set_time_out_div  CVWL568.lib(drv_dsi_tx.o)
    0x0001616c   0x0001616c   0x00000008   Code   RO         1864    i.drv_dsi_tx_set_video_chunk  CVWL568.lib(drv_dsi_tx.o)
    0x00016174   0x00016174   0x00000022   Code   RO         1865    i.drv_dsi_tx_set_video_timing  CVWL568.lib(drv_dsi_tx.o)
    0x00016196   0x00016196   0x00000008   Code   RO         1867    i.drv_dsi_tx_shutdown  CVWL568.lib(drv_dsi_tx.o)
    0x0001619e   0x0001619e   0x00000026   Code   RO         1868    i.drv_dsi_tx_timeout_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x000161c4   0x000161c4   0x000000aa   Code   RO         1871    i.drv_dsi_tx_video_mode_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x0001626e   0x0001626e   0x00000016   Code   RO         1872    i.drv_dsi_tx_video_mode_disable_hact_cmd  CVWL568.lib(drv_dsi_tx.o)
    0x00016284   0x00016284   0x00000018   Code   RO         1873    i.drv_dsi_tx_video_mode_set_lp_cmd  CVWL568.lib(drv_dsi_tx.o)
    0x0001629c   0x0001629c   0x0000002e   Code   RO         2272    i.drv_efuse_enter_inactive  CVWL568.lib(drv_efuse.o)
    0x000162ca   0x000162ca   0x0000000c   Code   RO         2275    i.drv_efuse_int_enable  CVWL568.lib(drv_efuse.o)
    0x000162d6   0x000162d6   0x00000032   Code   RO         2276    i.drv_efuse_read    CVWL568.lib(drv_efuse.o)
    0x00016308   0x00016308   0x00000018   Code   RO         2277    i.drv_efuse_read_req  CVWL568.lib(drv_efuse.o)
    0x00016320   0x00016320   0x00000018   Code   RO         1450    i.drv_gpio_get_input_data  CVWL568.lib(drv_gpio.o)
    0x00016338   0x00016338   0x0000000c   Code   RO         1452    i.drv_gpio_register_ap_reset_callback  CVWL568.lib(drv_gpio.o)
    0x00016344   0x00016344   0x00000014   Code   RO         1453    i.drv_gpio_register_callback  CVWL568.lib(drv_gpio.o)
    0x00016358   0x00016358   0x00000050   Code   RO         1455    i.drv_gpio_set_int  CVWL568.lib(drv_gpio.o)
    0x000163a8   0x000163a8   0x00000020   Code   RO         1456    i.drv_gpio_set_ioe  CVWL568.lib(drv_gpio.o)
    0x000163c8   0x000163c8   0x00000010   Code   RO         1457    i.drv_gpio_set_mode0  CVWL568.lib(drv_gpio.o)
    0x000163d8   0x000163d8   0x00000010   Code   RO         1458    i.drv_gpio_set_mode1  CVWL568.lib(drv_gpio.o)
    0x000163e8   0x000163e8   0x00000010   Code   RO         1459    i.drv_gpio_set_mode2  CVWL568.lib(drv_gpio.o)
    0x000163f8   0x000163f8   0x00000010   Code   RO         1460    i.drv_gpio_set_mode3  CVWL568.lib(drv_gpio.o)
    0x00016408   0x00016408   0x00000020   Code   RO          744    i.drv_gpio_set_output_data  CVWL568.lib(hal_gpio.o)
    0x00016428   0x00016428   0x00000130   Code   RO         1461    i.drv_gpio_set_pull_state  CVWL568.lib(drv_gpio.o)
    0x00016558   0x00016558   0x0000000c   Code   RO         1553    i.drv_i2c0_set_callback  CVWL568.lib(drv_i2c_slave.o)
    0x00016564   0x00016564   0x0000000c   Code   RO         1519    i.drv_i2c1_set_callback  CVWL568.lib(drv_i2c_master.o)
    0x00016570   0x00016570   0x00000034   Code   RO         1493    i.drv_i2c_dma_callback  CVWL568.lib(drv_i2c_dma.o)
    0x000165a4   0x000165a4   0x000000ac   Code   RO         1494    i.drv_i2c_dma_init  CVWL568.lib(drv_i2c_dma.o)
    0x00016650   0x00016650   0x0000001a   Code   RO         1495    i.drv_i2c_enable_rx_dma  CVWL568.lib(drv_i2c_dma.o)
    0x0001666a   0x0001666a   0x00000018   Code   RO         1496    i.drv_i2c_enable_tx_dma  CVWL568.lib(drv_i2c_dma.o)
    0x00016682   0x00016682   0x00000002   PAD
    0x00016684   0x00016684   0x00000060   Code   RO         1521    i.drv_i2c_m_clear_it_pending_bit  CVWL568.lib(drv_i2c_master.o)
    0x000166e4   0x000166e4   0x00000010   Code   RO         1524    i.drv_i2c_m_enable  CVWL568.lib(drv_i2c_master.o)
    0x000166f4   0x000166f4   0x00000038   Code   RO         1525    i.drv_i2c_m_enable_intr  CVWL568.lib(drv_i2c_master.o)
    0x0001672c   0x0001672c   0x0000008c   Code   RO         1531    i.drv_i2c_master_init  CVWL568.lib(drv_i2c_master.o)
    0x000167b8   0x000167b8   0x0000005c   Code   RO         1497    i.drv_i2c_master_read_dma  CVWL568.lib(drv_i2c_dma.o)
    0x00016814   0x00016814   0x0000003c   Code   RO         1498    i.drv_i2c_master_write_dma  CVWL568.lib(drv_i2c_dma.o)
    0x00016850   0x00016850   0x0000003e   Code   RO         1499    i.drv_i2c_master_write_read_cmd  CVWL568.lib(drv_i2c_dma.o)
    0x0001688e   0x0001688e   0x00000042   Code   RO         1554    i.drv_i2c_s_clear_it_pending_bit  CVWL568.lib(drv_i2c_slave.o)
    0x000168d0   0x000168d0   0x00000004   Code   RO         1555    i.drv_i2c_s_config_intr  CVWL568.lib(drv_i2c_slave.o)
    0x000168d4   0x000168d4   0x00000008   Code   RO         1556    i.drv_i2c_s_enable  CVWL568.lib(drv_i2c_slave.o)
    0x000168dc   0x000168dc   0x00000014   Code   RO         1557    i.drv_i2c_s_get_fifo_status  CVWL568.lib(drv_i2c_slave.o)
    0x000168f0   0x000168f0   0x00000050   Code   RO         1560    i.drv_i2c_s_set_intr  CVWL568.lib(drv_i2c_slave.o)
    0x00016940   0x00016940   0x0000001c   Code   RO         1561    i.drv_i2c_s_write_data  CVWL568.lib(drv_i2c_slave.o)
    0x0001695c   0x0001695c   0x00000058   Code   RO         1500    i.drv_i2c_set_dma_irq_callback  CVWL568.lib(drv_i2c_dma.o)
    0x000169b4   0x000169b4   0x00000032   Code   RO         1562    i.drv_i2c_slave_init  CVWL568.lib(drv_i2c_slave.o)
    0x000169e6   0x000169e6   0x00000002   PAD
    0x000169e8   0x000169e8   0x00000018   Code   RO         1501    i.drv_i2c_slave_write_dma  CVWL568.lib(drv_i2c_dma.o)
    0x00016a00   0x00016a00   0x00000018   Code   RO         1940    i.drv_lcdc_config_bypass  CVWL568.lib(drv_lcdc.o)
    0x00016a18   0x00016a18   0x00000030   Code   RO         1941    i.drv_lcdc_config_ccm  CVWL568.lib(drv_lcdc.o)
    0x00016a48   0x00016a48   0x00000016   Code   RO         1942    i.drv_lcdc_config_disp_mode  CVWL568.lib(drv_lcdc.o)
    0x00016a5e   0x00016a5e   0x00000024   Code   RO         1943    i.drv_lcdc_config_dpi_polarity  CVWL568.lib(drv_lcdc.o)
    0x00016a82   0x00016a82   0x00000026   Code   RO         1944    i.drv_lcdc_config_dpi_timing  CVWL568.lib(drv_lcdc.o)
    0x00016aa8   0x00016aa8   0x00000016   Code   RO         1945    i.drv_lcdc_config_edpi_mode  CVWL568.lib(drv_lcdc.o)
    0x00016abe   0x00016abe   0x00000016   Code   RO         1946    i.drv_lcdc_config_endianness  CVWL568.lib(drv_lcdc.o)
    0x00016ad4   0x00016ad4   0x0000000c   Code   RO         1947    i.drv_lcdc_config_input_size  CVWL568.lib(drv_lcdc.o)
    0x00016ae0   0x00016ae0   0x0000001e   Code   RO         1948    i.drv_lcdc_config_int  CVWL568.lib(drv_lcdc.o)
    0x00016afe   0x00016afe   0x00000022   Code   RO         1949    i.drv_lcdc_config_int_single  CVWL568.lib(drv_lcdc.o)
    0x00016b20   0x00016b20   0x00000022   Code   RO         1950    i.drv_lcdc_config_overwrite  CVWL568.lib(drv_lcdc.o)
    0x00016b42   0x00016b42   0x0000000c   Code   RO         1951    i.drv_lcdc_config_overwrite_rgb  CVWL568.lib(drv_lcdc.o)
    0x00016b4e   0x00016b4e   0x0000001a   Code   RO         1952    i.drv_lcdc_config_partial_display_area  CVWL568.lib(drv_lcdc.o)
    0x00016b68   0x00016b68   0x00000022   Code   RO         1953    i.drv_lcdc_config_partial_display_enable  CVWL568.lib(drv_lcdc.o)
    0x00016b8a   0x00016b8a   0x0000001a   Code   RO         1955    i.drv_lcdc_config_scale_up_coef  CVWL568.lib(drv_lcdc.o)
    0x00016ba4   0x00016ba4   0x0000000c   Code   RO         1956    i.drv_lcdc_config_scale_up_step  CVWL568.lib(drv_lcdc.o)
    0x00016bb0   0x00016bb0   0x0000004c   Code   RO         1957    i.drv_lcdc_config_src_parameter  CVWL568.lib(drv_lcdc.o)
    0x00016bfc   0x00016bfc   0x00000006   Code   RO         1958    i.drv_lcdc_config_thresh  CVWL568.lib(drv_lcdc.o)
    0x00016c02   0x00016c02   0x00000012   Code   RO         1959    i.drv_lcdc_ctrl_flow  CVWL568.lib(drv_lcdc.o)
    0x00016c14   0x00016c14   0x00000020   Code   RO         1961    i.drv_lcdc_enable_shadow_reg  CVWL568.lib(drv_lcdc.o)
    0x00016c34   0x00016c34   0x00000040   Code   RO         1962    i.drv_lcdc_set_int  CVWL568.lib(drv_lcdc.o)
    0x00016c74   0x00016c74   0x00000018   Code   RO         1963    i.drv_lcdc_set_prefetch  CVWL568.lib(drv_lcdc.o)
    0x00016c8c   0x00016c8c   0x00000014   Code   RO         1964    i.drv_lcdc_set_video_hw_mode  CVWL568.lib(drv_lcdc.o)
    0x00016ca0   0x00016ca0   0x00000020   Code   RO         1965    i.drv_lcdc_start    CVWL568.lib(drv_lcdc.o)
    0x00016cc0   0x00016cc0   0x0000000c   Code   RO         1999    i.drv_memc_clear_status  CVWL568.lib(drv_memc.o)
    0x00016ccc   0x00016ccc   0x00000040   Code   RO         2000    i.drv_memc_enable_irq  CVWL568.lib(drv_memc.o)
    0x00016d0c   0x00016d0c   0x0000000c   Code   RO         2001    i.drv_memc_gen_a_tear_signal  CVWL568.lib(drv_memc.o)
    0x00016d18   0x00016d18   0x00000012   Code   RO         2002    i.drv_memc_get_status  CVWL568.lib(drv_memc.o)
    0x00016d2a   0x00016d2a   0x00000010   Code   RO         2003    i.drv_memc_rate_transfer_sel  CVWL568.lib(drv_memc.o)
    0x00016d3a   0x00016d3a   0x0000000e   Code   RO         2004    i.drv_memc_sel_vsync  CVWL568.lib(drv_memc.o)
    0x00016d48   0x00016d48   0x00000014   Code   RO         2005    i.drv_memc_set_active_height  CVWL568.lib(drv_memc.o)
    0x00016d5c   0x00016d5c   0x0000000c   Code   RO         2006    i.drv_memc_set_data_mode  CVWL568.lib(drv_memc.o)
    0x00016d68   0x00016d68   0x00000010   Code   RO         2009    i.drv_memc_set_double_buffer  CVWL568.lib(drv_memc.o)
    0x00016d78   0x00016d78   0x00000012   Code   RO         2010    i.drv_memc_set_double_buffer_reverse  CVWL568.lib(drv_memc.o)
    0x00016d8a   0x00016d8a   0x00000010   Code   RO         2012    i.drv_memc_set_fs_en_conditions  CVWL568.lib(drv_memc.o)
    0x00016d9a   0x00016d9a   0x00000014   Code   RO         2013    i.drv_memc_set_inten  CVWL568.lib(drv_memc.o)
    0x00016dae   0x00016dae   0x00000002   PAD
    0x00016db0   0x00016db0   0x00000018   Code   RO         2014    i.drv_memc_set_lcdc_st_conditions  CVWL568.lib(drv_memc.o)
    0x00016dc8   0x00016dc8   0x0000001a   Code   RO         2015    i.drv_memc_set_ltpo_mode  CVWL568.lib(drv_memc.o)
    0x00016de2   0x00016de2   0x0000000e   Code   RO         2019    i.drv_memc_set_tear_mode  CVWL568.lib(drv_memc.o)
    0x00016df0   0x00016df0   0x00000028   Code   RO         2020    i.drv_memc_set_tear_waveform  CVWL568.lib(drv_memc.o)
    0x00016e18   0x00016e18   0x0000000e   Code   RO         2022    i.drv_memc_set_vidc_sync_cnt  CVWL568.lib(drv_memc.o)
    0x00016e26   0x00016e26   0x00000002   PAD
    0x00016e28   0x00016e28   0x00000008   Code   RO         1579    i.drv_param_init_get_ccm  CVWL568.lib(drv_param_init.o)
    0x00016e30   0x00016e30   0x00000014   Code   RO         1580    i.drv_param_init_get_scld_filter_h  CVWL568.lib(drv_param_init.o)
    0x00016e44   0x00016e44   0x00000014   Code   RO         1581    i.drv_param_init_get_scld_filter_v  CVWL568.lib(drv_param_init.o)
    0x00016e58   0x00016e58   0x00000008   Code   RO         1582    i.drv_param_init_get_sclu_filter  CVWL568.lib(drv_param_init.o)
    0x00016e60   0x00016e60   0x00000014   Code   RO         1583    i.drv_param_init_set_ccm  CVWL568.lib(drv_param_init.o)
    0x00016e74   0x00016e74   0x00000024   Code   RO         1586    i.drv_param_p2r_filter_init  CVWL568.lib(drv_param_init.o)
    0x00016e98   0x00016e98   0x00000010   Code   RO         2293    i.drv_phy_enable_calibration  CVWL568.lib(drv_phy_common.o)
    0x00016ea8   0x00016ea8   0x0000003c   Code   RO         2294    i.drv_phy_get_calibration  CVWL568.lib(drv_phy_common.o)
    0x00016ee4   0x00016ee4   0x00000060   Code   RO         2295    i.drv_phy_get_pll_para  CVWL568.lib(drv_phy_common.o)
    0x00016f44   0x00016f44   0x00000054   Code   RO         2296    i.drv_phy_get_rate_para  CVWL568.lib(drv_phy_common.o)
    0x00016f98   0x00016f98   0x00000010   Code   RO         2297    i.drv_phy_test_clear  CVWL568.lib(drv_phy_common.o)
    0x00016fa8   0x00016fa8   0x00000018   Code   RO         2298    i.drv_phy_test_lock  CVWL568.lib(drv_phy_common.o)
    0x00016fc0   0x00016fc0   0x00000020   Code   RO         2300    i.drv_phy_test_write_1_byte  CVWL568.lib(drv_phy_common.o)
    0x00016fe0   0x00016fe0   0x00000026   Code   RO         2301    i.drv_phy_test_write_2_byte  CVWL568.lib(drv_phy_common.o)
    0x00017006   0x00017006   0x0000001e   Code   RO         2302    i.drv_phy_test_write_code  CVWL568.lib(drv_phy_common.o)
    0x00017024   0x00017024   0x00000020   Code   RO         2303    i.drv_phy_test_write_data  CVWL568.lib(drv_phy_common.o)
    0x00017044   0x00017044   0x00000020   Code   RO         1602    i.drv_pwr_set_cp_mode  CVWL568.lib(drv_pwr.o)
    0x00017064   0x00017064   0x00000018   Code   RO         1604    i.drv_pwr_set_pvd_mode  CVWL568.lib(drv_pwr.o)
    0x0001707c   0x0001707c   0x00000038   Code   RO         1605    i.drv_pwr_set_system_clk_src  CVWL568.lib(drv_pwr.o)
    0x000170b4   0x000170b4   0x0000000c   Code   RO         1791    i.drv_rx_phy_test_clear  CVWL568.lib(drv_dsi_rx.o)
    0x000170c0   0x000170c0   0x00000010   Code   RO         1792    i.drv_rx_phy_test_lock  CVWL568.lib(drv_dsi_rx.o)
    0x000170d0   0x000170d0   0x00000014   Code   RO         1794    i.drv_rx_phy_test_write_1_byte  CVWL568.lib(drv_dsi_rx.o)
    0x000170e4   0x000170e4   0x00000016   Code   RO         1795    i.drv_rx_phy_test_write_2_byte  CVWL568.lib(drv_dsi_rx.o)
    0x000170fa   0x000170fa   0x0000000a   Code   RO         2058    i.drv_rxbr_clear_pkt_buffer  CVWL568.lib(drv_rxbr.o)
    0x00017104   0x00017104   0x00000004   Code   RO         2059    i.drv_rxbr_clear_status0  CVWL568.lib(drv_rxbr.o)
    0x00017108   0x00017108   0x0000005a   Code   RO         2061    i.drv_rxbr_enable_irq  CVWL568.lib(drv_rxbr.o)
    0x00017162   0x00017162   0x00000002   PAD
    0x00017164   0x00017164   0x00000014   Code   RO         2062    i.drv_rxbr_frame_drop_cfg  CVWL568.lib(drv_rxbr.o)
    0x00017178   0x00017178   0x00000064   Code   RO         2063    i.drv_rxbr_get_clk  CVWL568.lib(drv_rxbr.o)
    0x000171dc   0x000171dc   0x00000004   Code   RO         2064    i.drv_rxbr_get_col_addr  CVWL568.lib(drv_rxbr.o)
    0x000171e0   0x000171e0   0x00000012   Code   RO         1098    i.drv_rxbr_get_int_source  CVWL568.lib(hal_internal_vsync.o)
    0x000171f2   0x000171f2   0x00000004   Code   RO         2067    i.drv_rxbr_get_page_addr  CVWL568.lib(drv_rxbr.o)
    0x000171f6   0x000171f6   0x00000012   Code   RO         1099    i.drv_rxbr_get_status0  CVWL568.lib(hal_internal_vsync.o)
    0x00017208   0x00017208   0x0000000c   Code   RO         2069    i.drv_rxbr_hline_rcv0_cfg  CVWL568.lib(drv_rxbr.o)
    0x00017214   0x00017214   0x00000008   Code   RO         2070    i.drv_rxbr_hline_rcv_cfg  CVWL568.lib(drv_rxbr.o)
    0x0001721c   0x0001721c   0x0000000c   Code   RO         2071    i.drv_rxbr_register_irq0_callback  CVWL568.lib(drv_rxbr.o)
    0x00017228   0x00017228   0x0000000c   Code   RO         2072    i.drv_rxbr_register_irq1_callback  CVWL568.lib(drv_rxbr.o)
    0x00017234   0x00017234   0x00000014   Code   RO         2073    i.drv_rxbr_set_ack_pkt_header  CVWL568.lib(drv_rxbr.o)
    0x00017248   0x00017248   0x000000cc   Code   RO         2074    i.drv_rxbr_set_cmd_filter  CVWL568.lib(drv_rxbr.o)
    0x00017314   0x00017314   0x00000014   Code   RO         2076    i.drv_rxbr_set_color_format  CVWL568.lib(drv_rxbr.o)
    0x00017328   0x00017328   0x00000014   Code   RO         2078    i.drv_rxbr_set_inten  CVWL568.lib(drv_rxbr.o)
    0x0001733c   0x0001733c   0x00000010   Code   RO         2079    i.drv_rxbr_set_ltpo_drop_th  CVWL568.lib(drv_rxbr.o)
    0x0001734c   0x0001734c   0x00000026   Code   RO         2081    i.drv_rxbr_set_usr_cfg  CVWL568.lib(drv_rxbr.o)
    0x00017372   0x00017372   0x00000008   Code   RO         2082    i.drv_rxbr_set_usr_col  CVWL568.lib(drv_rxbr.o)
    0x0001737a   0x0001737a   0x00000008   Code   RO         2083    i.drv_rxbr_set_usr_row  CVWL568.lib(drv_rxbr.o)
    0x00017382   0x00017382   0x00000002   PAD
    0x00017384   0x00017384   0x00000020   Code   RO         1650    i.drv_spi_m_read_data  CVWL568.lib(drv_spi_master.o)
    0x000173a4   0x000173a4   0x00000054   Code   RO         1678    i.drv_swire_set_int  CVWL568.lib(drv_swire.o)
    0x000173f8   0x000173f8   0x0000001c   Code   RO         1679    i.drv_swire_set_power_down  CVWL568.lib(drv_swire.o)
    0x00017414   0x00017414   0x0000000c   Code   RO         1694    i.drv_sys_cfg_clear_all_int  CVWL568.lib(drv_sys_cfg.o)
    0x00017420   0x00017420   0x00000028   Code   RO         1695    i.drv_sys_cfg_clear_pending  CVWL568.lib(drv_sys_cfg.o)
    0x00017448   0x00017448   0x00000018   Code   RO         1698    i.drv_sys_cfg_sel_ap_rst_lvl_trig  CVWL568.lib(drv_sys_cfg.o)
    0x00017460   0x00017460   0x0000001c   Code   RO         1699    i.drv_sys_cfg_sel_ap_rst_trig  CVWL568.lib(drv_sys_cfg.o)
    0x0001747c   0x0001747c   0x00000024   Code   RO         1700    i.drv_sys_cfg_sel_gpio_group  CVWL568.lib(drv_sys_cfg.o)
    0x000174a0   0x000174a0   0x00000024   Code   RO         1701    i.drv_sys_cfg_sel_int_trig  CVWL568.lib(drv_sys_cfg.o)
    0x000174c4   0x000174c4   0x00000010   Code   RO         1703    i.drv_sys_cfg_set_dma_rx_req  CVWL568.lib(drv_sys_cfg.o)
    0x000174d4   0x000174d4   0x00000010   Code   RO         1704    i.drv_sys_cfg_set_dma_tx_req  CVWL568.lib(drv_sys_cfg.o)
    0x000174e4   0x000174e4   0x00000024   Code   RO         1705    i.drv_sys_cfg_set_int  CVWL568.lib(drv_sys_cfg.o)
    0x00017508   0x00017508   0x0000001a   Code   RO         1728    i.drv_timer_clear_status_flags  CVWL568.lib(drv_timer.o)
    0x00017522   0x00017522   0x00000020   Code   RO         1729    i.drv_timer_enable  CVWL568.lib(drv_timer.o)
    0x00017542   0x00017542   0x00000002   PAD
    0x00017544   0x00017544   0x00000010   Code   RO         1730    i.drv_timer_get_instance  CVWL568.lib(drv_timer.o)
    0x00017554   0x00017554   0x00000010   Code   RO         1731    i.drv_timer_get_prescaler  CVWL568.lib(drv_timer.o)
    0x00017564   0x00017564   0x00000044   Code   RO         1733    i.drv_timer_handle_interrupt  CVWL568.lib(drv_timer.o)
    0x000175a8   0x000175a8   0x00000014   Code   RO         1734    i.drv_timer_register_callback  CVWL568.lib(drv_timer.o)
    0x000175bc   0x000175bc   0x00000010   Code   RO         1735    i.drv_timer_set_compare_val  CVWL568.lib(drv_timer.o)
    0x000175cc   0x000175cc   0x00000054   Code   RO         1736    i.drv_timer_set_int  CVWL568.lib(drv_timer.o)
    0x00017620   0x00017620   0x00000028   Code   RO         1737    i.drv_timer_set_prescaler  CVWL568.lib(drv_timer.o)
    0x00017648   0x00017648   0x0000000a   Code   RO         1874    i.drv_tx_phy_test_clear  CVWL568.lib(drv_dsi_tx.o)
    0x00017652   0x00017652   0x0000001c   Code   RO         1875    i.drv_tx_phy_test_enter  CVWL568.lib(drv_dsi_tx.o)
    0x0001766e   0x0001766e   0x0000001c   Code   RO         1876    i.drv_tx_phy_test_exit  CVWL568.lib(drv_dsi_tx.o)
    0x0001768a   0x0001768a   0x00000012   Code   RO         1878    i.drv_tx_phy_test_write_1_byte  CVWL568.lib(drv_dsi_tx.o)
    0x0001769c   0x0001769c   0x00000014   Code   RO         1879    i.drv_tx_phy_test_write_2_byte  CVWL568.lib(drv_dsi_tx.o)
    0x000176b0   0x000176b0   0x00000010   Code   RO         1880    i.drv_tx_phy_test_write_code  CVWL568.lib(drv_dsi_tx.o)
    0x000176c0   0x000176c0   0x00000008   Code   RO         2122    i.drv_vidc_clear_irq  CVWL568.lib(drv_vidc.o)
    0x000176c8   0x000176c8   0x00000018   Code   RO         2126    i.drv_vidc_enable   CVWL568.lib(drv_vidc.o)
    0x000176e0   0x000176e0   0x00000040   Code   RO         2127    i.drv_vidc_enable_irq  CVWL568.lib(drv_vidc.o)
    0x00017720   0x00017720   0x00000012   Code   RO         2129    i.drv_vidc_get_irq_status  CVWL568.lib(drv_vidc.o)
    0x00017732   0x00017732   0x00000002   PAD
    0x00017734   0x00017734   0x00000028   Code   RO         2133    i.drv_vidc_init_module_enable  CVWL568.lib(drv_vidc.o)
    0x0001775c   0x0001775c   0x0000000c   Code   RO         2134    i.drv_vidc_register_callback  CVWL568.lib(drv_vidc.o)
    0x00017768   0x00017768   0x00000006   Code   RO         2135    i.drv_vidc_reset    CVWL568.lib(drv_vidc.o)
    0x0001776e   0x0001776e   0x0000003c   Code   RO         2137    i.drv_vidc_set_dst_parameter  CVWL568.lib(drv_vidc.o)
    0x000177aa   0x000177aa   0x00000014   Code   RO         2141    i.drv_vidc_set_irqen  CVWL568.lib(drv_vidc.o)
    0x000177be   0x000177be   0x00000010   Code   RO         2142    i.drv_vidc_set_mirror  CVWL568.lib(drv_vidc.o)
    0x000177ce   0x000177ce   0x00000008   Code   RO         2145    i.drv_vidc_set_p2r_hcoef0  CVWL568.lib(drv_vidc.o)
    0x000177d6   0x000177d6   0x00000026   Code   RO         2146    i.drv_vidc_set_p2r_hinitb  CVWL568.lib(drv_vidc.o)
    0x000177fc   0x000177fc   0x00000026   Code   RO         2147    i.drv_vidc_set_p2r_hinitr  CVWL568.lib(drv_vidc.o)
    0x00017822   0x00017822   0x00000002   PAD
    0x00017824   0x00017824   0x00000018   Code   RO         2148    i.drv_vidc_set_pentile_swap  CVWL568.lib(drv_vidc.o)
    0x0001783c   0x0001783c   0x0000000a   Code   RO         2149    i.drv_vidc_set_pu_ctrl  CVWL568.lib(drv_vidc.o)
    0x00017846   0x00017846   0x00000010   Code   RO         2150    i.drv_vidc_set_rotation  CVWL568.lib(drv_vidc.o)
    0x00017856   0x00017856   0x0000000a   Code   RO         2151    i.drv_vidc_set_scld_hcoef0  CVWL568.lib(drv_vidc.o)
    0x00017860   0x00017860   0x0000000a   Code   RO         2152    i.drv_vidc_set_scld_hcoef1  CVWL568.lib(drv_vidc.o)
    0x0001786a   0x0001786a   0x00000012   Code   RO         2153    i.drv_vidc_set_scld_step  CVWL568.lib(drv_vidc.o)
    0x0001787c   0x0001787c   0x0000000a   Code   RO         2154    i.drv_vidc_set_scld_vcoef0  CVWL568.lib(drv_vidc.o)
    0x00017886   0x00017886   0x0000000a   Code   RO         2155    i.drv_vidc_set_scld_vcoef1  CVWL568.lib(drv_vidc.o)
    0x00017890   0x00017890   0x00000016   Code   RO         2156    i.drv_vidc_set_src_parameter  CVWL568.lib(drv_vidc.o)
    0x000178a6   0x000178a6   0x00000002   PAD
    0x000178a8   0x000178a8   0x00000010   Code   RO         2745    i.drv_wdg_clear_counter  CVWL568.lib(drv_wdg.o)
    0x000178b8   0x000178b8   0x00000010   Code   RO         2746    i.drv_wdg_clear_edge_flag  CVWL568.lib(drv_wdg.o)
    0x000178c8   0x000178c8   0x00000010   Code   RO         2749    i.drv_wdg_read_edge_flag  CVWL568.lib(drv_wdg.o)
    0x000178d8   0x000178d8   0x00000040   Code   RO         2752    i.drv_wdg_set_int   CVWL568.lib(drv_wdg.o)
    0x00017918   0x00017918   0x0000000a   Code   RO         1362    i.fls_clr_interrupt_flag  CVWL568.lib(drv_fls.o)
    0x00017922   0x00017922   0x00000014   Code   RO         2352    i.fputc             CVWL568.lib(tau_log.o)
    0x00017936   0x00017936   0x00000002   PAD
    0x00017938   0x00017938   0x00000034   Code   RO          547    i.hal_dsi_rx_ctrl_create_handle  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001796c   0x0001796c   0x0000009c   Code   RO          549    i.hal_dsi_rx_ctrl_deinit  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017a08   0x00017a08   0x00000084   Code   RO          551    i.hal_dsi_rx_ctrl_dsc_async_handler  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017a8c   0x00017a8c   0x00000028   Code   RO          553    i.hal_dsi_rx_ctrl_gen_a_tear_signal  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017ab4   0x00017ab4   0x00000028   Code   RO          555    i.hal_dsi_rx_ctrl_get_max_ret_size  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017adc   0x00017adc   0x00000064   Code   RO          556    i.hal_dsi_rx_ctrl_hight_performan_mode  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017b40   0x00017b40   0x00000098   Code   RO          557    i.hal_dsi_rx_ctrl_init  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017bd8   0x00017bd8   0x000001a4   Code   RO          558    i.hal_dsi_rx_ctrl_init_clk  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017d7c   0x00017d7c   0x000000d8   Code   RO          559    i.hal_dsi_rx_ctrl_init_dsi_rx  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017e54   0x00017e54   0x00000158   Code   RO          560    i.hal_dsi_rx_ctrl_init_memc  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017fac   0x00017fac   0x00000148   Code   RO          561    i.hal_dsi_rx_ctrl_init_rxbr  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000180f4   0x000180f4   0x0000022c   Code   RO          562    i.hal_dsi_rx_ctrl_init_vidc  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00018320   0x00018320   0x0000003c   Code   RO          563    i.hal_dsi_rx_ctrl_pre_init_pps  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001835c   0x0001835c   0x000000f0   Code   RO          566    i.hal_dsi_rx_ctrl_send_ack_cmd  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001844c   0x0001844c   0x00000034   Code   RO          570    i.hal_dsi_rx_ctrl_set_cus_sync_line  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00018480   0x00018480   0x00000034   Code   RO          573    i.hal_dsi_rx_ctrl_set_hw_tear_mode  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000184b4   0x000184b4   0x00000038   Code   RO          574    i.hal_dsi_rx_ctrl_set_ipi_cfg  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000184ec   0x000184ec   0x00000072   Code   RO          579    i.hal_dsi_rx_ctrl_set_rxbr_clk  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001855e   0x0001855e   0x00000002   PAD
    0x00018560   0x00018560   0x00000034   Code   RO          580    i.hal_dsi_rx_ctrl_set_sw_tear_mode  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00018594   0x00018594   0x0000000e   Code   RO          582    i.hal_dsi_rx_ctrl_set_tear_mode_ex  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000185a2   0x000185a2   0x00000002   PAD
    0x000185a4   0x000185a4   0x0000003c   Code   RO          583    i.hal_dsi_rx_ctrl_start  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000185e0   0x000185e0   0x0000003c   Code   RO          584    i.hal_dsi_rx_ctrl_stop  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001861c   0x0001861c   0x00000020   Code   RO          586    i.hal_dsi_rx_ctrl_toggle_resolution  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001863c   0x0001863c   0x00000190   Code   RO          640    i.hal_dsi_tx_calc_video_chunks  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000187cc   0x000187cc   0x00000034   Code   RO          641    i.hal_dsi_tx_config_params_for_lane_rate  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018800   0x00018800   0x00000450   Code   RO          642    i.hal_dsi_tx_count_lane_rate  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018c50   0x00018c50   0x0000002c   Code   RO          645    i.hal_dsi_tx_ctrl_create_handle  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018c7c   0x00018c7c   0x00000084   Code   RO          646    i.hal_dsi_tx_ctrl_deinit  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018d00   0x00018d00   0x0000004c   Code   RO          650    i.hal_dsi_tx_ctrl_enter_init_panel_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018d4c   0x00018d4c   0x00000028   Code   RO          652    i.hal_dsi_tx_ctrl_exit_init_panel_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018d74   0x00018d74   0x000000a4   Code   RO          654    i.hal_dsi_tx_ctrl_init  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018e18   0x00018e18   0x00000024   Code   RO          655    i.hal_dsi_tx_ctrl_init_clk  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018e3c   0x00018e3c   0x0000000c   Code   RO          656    i.hal_dsi_tx_ctrl_panel_reset_pin  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018e48   0x00018e48   0x00000020   Code   RO          659    i.hal_dsi_tx_ctrl_set_ccm  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018e68   0x00018e68   0x00000014   Code   RO          665    i.hal_dsi_tx_ctrl_set_overwrite_rgb  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018e7c   0x00018e7c   0x00000010   Code   RO          666    i.hal_dsi_tx_ctrl_set_partial_disp  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018e8c   0x00018e8c   0x00000024   Code   RO          667    i.hal_dsi_tx_ctrl_set_partial_disp_area  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018eb0   0x00018eb0   0x0000009c   Code   RO          670    i.hal_dsi_tx_ctrl_start  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018f4c   0x00018f4c   0x00000044   Code   RO          671    i.hal_dsi_tx_ctrl_stop  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018f90   0x00018f90   0x000000d8   Code   RO          672    i.hal_dsi_tx_ctrl_write_array_cmd  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00019068   0x00019068   0x000000b0   Code   RO          673    i.hal_dsi_tx_ctrl_write_cmd  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00019118   0x00019118   0x00000044   Code   RO          674    i.hal_dsi_tx_init_data_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001915c   0x0001915c   0x00000030   Code   RO          675    i.hal_dsi_tx_init_dpi_cfg  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001918c   0x0001918c   0x00000020   Code   RO          676    i.hal_dsi_tx_init_interrupt  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000191ac   0x000191ac   0x00000020   Code   RO          677    i.hal_dsi_tx_init_phy_cfg  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000191cc   0x000191cc   0x00000094   Code   RO          678    i.hal_dsi_tx_init_remains  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00019260   0x00019260   0x00000058   Code   RO          679    i.hal_dsi_tx_init_video_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000192b8   0x000192b8   0x00000044   Code   RO          680    i.hal_dsi_tx_send_cmd  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000192fc   0x000192fc   0x00000018   Code   RO          745    i.hal_gpio_ctrl_eint  CVWL568.lib(hal_gpio.o)
    0x00019314   0x00019314   0x00000012   Code   RO          746    i.hal_gpio_get_input_data  CVWL568.lib(hal_gpio.o)
    0x00019326   0x00019326   0x00000002   PAD
    0x00019328   0x00019328   0x00000040   Code   RO          749    i.hal_gpio_init_eint  CVWL568.lib(hal_gpio.o)
    0x00019368   0x00019368   0x00000020   Code   RO          750    i.hal_gpio_init_input  CVWL568.lib(hal_gpio.o)
    0x00019388   0x00019388   0x00000028   Code   RO          751    i.hal_gpio_init_output  CVWL568.lib(hal_gpio.o)
    0x000193b0   0x000193b0   0x00000018   Code   RO          752    i.hal_gpio_reg_eint_cb  CVWL568.lib(hal_gpio.o)
    0x000193c8   0x000193c8   0x00000050   Code   RO          753    i.hal_gpio_set_ap_reset_int  CVWL568.lib(hal_gpio.o)
    0x00019418   0x00019418   0x00000060   Code   RO          755    i.hal_gpio_set_mode  CVWL568.lib(hal_gpio.o)
    0x00019478   0x00019478   0x00000008   Code   RO          756    i.hal_gpio_set_output_data  CVWL568.lib(hal_gpio.o)
    0x00019480   0x00019480   0x00000020   Code   RO          758    i.hal_gpio_set_pull_state  CVWL568.lib(hal_gpio.o)
    0x000194a0   0x000194a0   0x0000006c   Code   RO          784    i.hal_i2c_m_dma_init  CVWL568.lib(hal_i2c_master.o)
    0x0001950c   0x0001950c   0x00000020   Code   RO          785    i.hal_i2c_m_dma_read  CVWL568.lib(hal_i2c_master.o)
    0x0001952c   0x0001952c   0x0000001c   Code   RO          786    i.hal_i2c_m_dma_write  CVWL568.lib(hal_i2c_master.o)
    0x00019548   0x00019548   0x0000000c   Code   RO          788    i.hal_i2c_m_transfer_complate  CVWL568.lib(hal_i2c_master.o)
    0x00019554   0x00019554   0x00000020   Code   RO          789    i.hal_i2c_master_irq_callback  CVWL568.lib(hal_i2c_master.o)
    0x00019574   0x00019574   0x00000010   Code   RO          803    i.hal_i2c_s_dma_user_callback  CVWL568.lib(hal_i2c_slave.o)
    0x00019584   0x00019584   0x0000004c   Code   RO          804    i.hal_i2c_s_dma_write  CVWL568.lib(hal_i2c_slave.o)
    0x000195d0   0x000195d0   0x000000c8   Code   RO          806    i.hal_i2c_s_init    CVWL568.lib(hal_i2c_slave.o)
    0x00019698   0x00019698   0x00000014   Code   RO          807    i.hal_i2c_s_nonblocking_read  CVWL568.lib(hal_i2c_slave.o)
    0x000196ac   0x000196ac   0x0000000c   Code   RO          815    i.hal_i2c_s_set_transfer  CVWL568.lib(hal_i2c_slave.o)
    0x000196b8   0x000196b8   0x00000174   Code   RO          818    i.hal_i2c_slave_irq_callback  CVWL568.lib(hal_i2c_slave.o)
    0x0001982c   0x0001982c   0x000000fc   Code   RO         1100    i.hal_internal_init_memc  CVWL568.lib(hal_internal_vsync.o)
    0x00019928   0x00019928   0x00000010   Code   RO         1102    i.hal_internal_sync_get_fb_setting  CVWL568.lib(hal_internal_vsync.o)
    0x00019938   0x00019938   0x00000010   Code   RO         1103    i.hal_internal_sync_get_hight_performan_mode  CVWL568.lib(hal_internal_vsync.o)
    0x00019948   0x00019948   0x0000022c   Code   RO         1104    i.hal_internal_sync_input_resolution_change  CVWL568.lib(hal_internal_vsync.o)
    0x00019b74   0x00019b74   0x00000010   Code   RO         1107    i.hal_internal_update_dpi_param  CVWL568.lib(hal_internal_vsync.o)
    0x00019b84   0x00019b84   0x0000012c   Code   RO         1108    i.hal_internal_video_mode_auto_sync  CVWL568.lib(hal_internal_vsync.o)
    0x00019cb0   0x00019cb0   0x00000028   Code   RO         1109    i.hal_internal_vsync_deinit  CVWL568.lib(hal_internal_vsync.o)
    0x00019cd8   0x00019cd8   0x0000000c   Code   RO         1110    i.hal_internal_vsync_get_rx_state  CVWL568.lib(hal_internal_vsync.o)
    0x00019ce4   0x00019ce4   0x00000018   Code   RO         1111    i.hal_internal_vsync_get_sync_line  CVWL568.lib(hal_internal_vsync.o)
    0x00019cfc   0x00019cfc   0x0000000c   Code   RO         1112    i.hal_internal_vsync_get_tear_mode  CVWL568.lib(hal_internal_vsync.o)
    0x00019d08   0x00019d08   0x0000000c   Code   RO         1113    i.hal_internal_vsync_get_tx_state  CVWL568.lib(hal_internal_vsync.o)
    0x00019d14   0x00019d14   0x00000118   Code   RO         1114    i.hal_internal_vsync_init_rx  CVWL568.lib(hal_internal_vsync.o)
    0x00019e2c   0x00019e2c   0x000000b0   Code   RO         1115    i.hal_internal_vsync_init_tx  CVWL568.lib(hal_internal_vsync.o)
    0x00019edc   0x00019edc   0x0000011c   Code   RO         1117    i.hal_internal_vsync_set_auto_hw_filter  CVWL568.lib(hal_internal_vsync.o)
    0x00019ff8   0x00019ff8   0x00000014   Code   RO         1119    i.hal_internal_vsync_set_rx_state  CVWL568.lib(hal_internal_vsync.o)
    0x0001a00c   0x0001a00c   0x00000024   Code   RO         1120    i.hal_internal_vsync_set_sync_line  CVWL568.lib(hal_internal_vsync.o)
    0x0001a030   0x0001a030   0x00000050   Code   RO         1121    i.hal_internal_vsync_set_tear_mode  CVWL568.lib(hal_internal_vsync.o)
    0x0001a080   0x0001a080   0x00000080   Code   RO         1122    i.hal_internal_vsync_set_tx_state  CVWL568.lib(hal_internal_vsync.o)
    0x0001a100   0x0001a100   0x00000024   Code   RO          681    i.hal_lcdc_config_ccm  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001a124   0x0001a124   0x00000058   Code   RO          682    i.hal_lcdc_config_remains  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001a17c   0x0001a17c   0x00000014   Code   RO          683    i.hal_lcdc_config_rgb_to_pentile  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001a190   0x0001a190   0x00000164   Code   RO          684    i.hal_lcdc_config_upscaler  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001a2f4   0x0001a2f4   0x00000054   Code   RO          685    i.hal_lcdc_init_cfg  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001a348   0x0001a348   0x000001b0   Code   RO          686    i.hal_lcdc_init_clk  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001a4f8   0x0001a4f8   0x00000040   Code   RO          687    i.hal_lcdc_init_interrupt  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001a538   0x0001a538   0x0000000e   Code   RO          843    i.hal_spi_m_clear_rxfifo  CVWL568.lib(hal_spi_master.o)
    0x0001a546   0x0001a546   0x00000016   Code   RO          869    i.hal_swire_open    CVWL568.lib(hal_swire.o)
    0x0001a55c   0x0001a55c   0x00000008   Code   RO          884    i.hal_system_enable_systick  CVWL568.lib(hal_system.o)
    0x0001a564   0x0001a564   0x00000088   Code   RO          888    i.hal_system_init   CVWL568.lib(hal_system.o)
    0x0001a5ec   0x0001a5ec   0x0000001c   Code   RO          889    i.hal_system_init_console  CVWL568.lib(hal_system.o)
    0x0001a608   0x0001a608   0x00000008   Code   RO          892    i.hal_system_set_phy_calibration  CVWL568.lib(hal_system.o)
    0x0001a610   0x0001a610   0x00000008   Code   RO          893    i.hal_system_set_pvd  CVWL568.lib(hal_system.o)
    0x0001a618   0x0001a618   0x00000008   Code   RO          894    i.hal_system_set_vcc  CVWL568.lib(hal_system.o)
    0x0001a620   0x0001a620   0x0000001a   Code   RO          919    i.hal_timer_init    CVWL568.lib(hal_timer.o)
    0x0001a63a   0x0001a63a   0x00000002   PAD
    0x0001a63c   0x0001a63c   0x00000048   Code   RO          921    i.hal_timer_start   CVWL568.lib(hal_timer.o)
    0x0001a684   0x0001a684   0x00000028   Code   RO          923    i.hal_timer_stop    CVWL568.lib(hal_timer.o)
    0x0001a6ac   0x0001a6ac   0x0000008c   Code   RO         1076    i.hal_uart_init     CVWL568.lib(hal_uart.o)
    0x0001a738   0x0001a738   0x00000010   Code   RO         1079    i.hal_uart_transmit_blocking  CVWL568.lib(hal_uart.o)
    0x0001a748   0x0001a748   0x00000110   Code   RO         2232    i.handle_init       CVWL568.lib(irq_redirect .o)
    0x0001a858   0x0001a858   0x00000064   Code   RO          117    i.init_mipi_tx      ap_demo.o
    0x0001a8bc   0x0001a8bc   0x00000088   Code   RO          118    i.init_panel        ap_demo.o
    0x0001a944   0x0001a944   0x0000000a   Code   RO            3    i.main              main.o
    0x0001a94e   0x0001a94e   0x00000002   PAD
    0x0001a950   0x0001a950   0x000000a0   Code   RO          119    i.open_mipi_rx      ap_demo.o
    0x0001a9f0   0x0001a9f0   0x00000054   Code   RO          120    i.pps_update_handle  ap_demo.o
    0x0001aa44   0x0001aa44   0x000003f4   Code   RO         1126    i.rx_get_dcs_packet_data  CVWL568.lib(hal_internal_vsync.o)
    0x0001ae38   0x0001ae38   0x00000178   Code   RO         1127    i.rx_partial_update  CVWL568.lib(hal_internal_vsync.o)
    0x0001afb0   0x0001afb0   0x0000008c   Code   RO         1128    i.rx_receive_packet  CVWL568.lib(hal_internal_vsync.o)
    0x0001b03c   0x0001b03c   0x00000180   Code   RO         1129    i.rx_receive_pps    CVWL568.lib(hal_internal_vsync.o)
    0x0001b1bc   0x0001b1bc   0x000000a4   Code   RO         1130    i.rxbr_irq0_callback  CVWL568.lib(hal_internal_vsync.o)
    0x0001b260   0x0001b260   0x000001dc   Code   RO         1131    i.rxbr_irq1_callback  CVWL568.lib(hal_internal_vsync.o)
    0x0001b43c   0x0001b43c   0x000000c4   Code   RO         1132    i.soft_gen_te       CVWL568.lib(hal_internal_vsync.o)
    0x0001b500   0x0001b500   0x000000c0   Code   RO         1133    i.soft_gen_te_double_buffer  CVWL568.lib(hal_internal_vsync.o)
    0x0001b5c0   0x0001b5c0   0x00000030   Code   RO          121    i.soft_timer3_cb    ap_demo.o
    0x0001b5f0   0x0001b5f0   0x00000048   Code   RO         2772    i.sqrt              m_ps.l(sqrt.o)
    0x0001b638   0x0001b638   0x00000040   Code   RO          122    i.tp_heartbeat_exec  ap_demo.o
    0x0001b678   0x0001b678   0x00000108   Code   RO         1134    i.vidc_callback     CVWL568.lib(hal_internal_vsync.o)
    0x0001b780   0x0001b780   0x000000d0   Code   RO         1135    i.vpre_err_reset    CVWL568.lib(hal_internal_vsync.o)
    0x0001b850   0x0001b850   0x000001cc   Code   RO         1136    i.vsync_set_te_mode  CVWL568.lib(hal_internal_vsync.o)
    0x0001ba1c   0x0001ba1c   0x000000f8   Data   RO          123    .constdata          ap_demo.o
    0x0001bb14   0x0001bb14   0x00000024   Data   RO          689    .constdata          CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001bb38   0x0001bb38   0x000000d2   Data   RO          761    .constdata          CVWL568.lib(hal_gpio.o)
    0x0001bc0a   0x0001bc0a   0x00000002   PAD
    0x0001bc0c   0x0001bc0c   0x00000020   Data   RO          819    .constdata          CVWL568.lib(hal_i2c_slave.o)
    0x0001bc2c   0x0001bc2c   0x00002150   Data   RO          947    .constdata          WL568_20U_HX667_TP.lib(app_tp_for_custom_s8.o)
    0x0001dd7c   0x0001dd7c   0x00000001   Data   RO          960    .constdata          WL568_20U_HX667_TP.lib(app_tp_for_custom_s8.o)
    0x0001dd7d   0x0001dd7d   0x00000003   PAD
    0x0001dd80   0x0001dd80   0x00000008   Data   RO         1587    .constdata          CVWL568.lib(drv_param_init.o)
    0x0001dd88   0x0001dd88   0x00000186   Data   RO         2304    .constdata          CVWL568.lib(drv_phy_common.o)
    0x0001df0e   0x0001df0e   0x00000002   PAD
    0x0001df10   0x0001df10   0x00000048   Data   RO          590    .conststring        CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001df58   0x0001df58   0x00000043   Data   RO          690    .conststring        CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001df9b   0x0001df9b   0x00000001   PAD
    0x0001df9c   0x0001df9c   0x00000134   Data   RO         1138    .conststring        CVWL568.lib(hal_internal_vsync.o)
    0x0001e0d0   0x0001e0d0   0x00000030   Data   RO         3134    Region$$Table       anon$$obj.o


    Execution Region RW_RAM1 (Exec base: 0x00070000, Load base: 0x0001e100, Size: 0x00000000, Max: 0x000000f0, ABSOLUTE)

    **** No section assigned to this execution region ****


    Execution Region RW_RAM2 (Exec base: 0x00070100, Load base: 0x0001e100, Size: 0x000000c0, Max: 0x000000d0, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00070100        -       0x000000c0   Zero   RW         2233    .ARM.__AT_0x00070100  CVWL568.lib(irq_redirect .o)


    Execution Region RW_RAM3 (Exec base: 0x000701d0, Load base: 0x0001e100, Size: 0x00005480, Max: 0x00007e30, ABSOLUTE, COMPRESSED[0x00001450])

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x000701d0   COMPRESSED   0x00001d66   Data   RW          124    .data               ap_demo.o
    0x00071f36   COMPRESSED   0x00000017   Data   RW          292    .data               app_tp_transfer.o
    0x00071f4d   COMPRESSED   0x00000028   Data   RW          431    .data               app_tp_st_touch.o
    0x00071f75   COMPRESSED   0x00000003   PAD
    0x00071f78   COMPRESSED   0x00000008   Data   RW          591    .data               CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00071f80   COMPRESSED   0x00000003   Data   RW          691    .data               CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00071f83   COMPRESSED   0x00000001   Data   RW          790    .data               CVWL568.lib(hal_i2c_master.o)
    0x00071f84   COMPRESSED   0x00000020   Data   RW          820    .data               CVWL568.lib(hal_i2c_slave.o)
    0x00071fa4   COMPRESSED   0x000000e4   Data   RW          961    .data               WL568_20U_HX667_TP.lib(app_tp_for_custom_s8.o)
    0x00072088   COMPRESSED   0x00000001   Data   RW          964    .data               WL568_20U_HX667_TP.lib(app_tp_for_custom_s8.o)
    0x00072089   COMPRESSED   0x00000001   Data   RW          965    .data               WL568_20U_HX667_TP.lib(app_tp_for_custom_s8.o)
    0x0007208a   COMPRESSED   0x00000001   Data   RW          970    .data               WL568_20U_HX667_TP.lib(app_tp_for_custom_s8.o)
    0x0007208b   COMPRESSED   0x00000003   Data   RW          971    .data               WL568_20U_HX667_TP.lib(app_tp_for_custom_s8.o)
    0x0007208e   COMPRESSED   0x00000005   Data   RW          972    .data               WL568_20U_HX667_TP.lib(app_tp_for_custom_s8.o)
    0x00072093   COMPRESSED   0x00000001   PAD
    0x00072094   COMPRESSED   0x00000030   Data   RW          982    .data               WL568_20U_HX667_TP.lib(app_tp_for_custom_s8.o)
    0x000720c4   COMPRESSED   0x00000018   Data   RW         1139    .data               CVWL568.lib(hal_internal_vsync.o)
    0x000720dc   COMPRESSED   0x0000000c   Data   RW         1198    .data               CVWL568.lib(drv_common.o)
    0x000720e8   COMPRESSED   0x00000004   Data   RW         1465    .data               CVWL568.lib(drv_gpio.o)
    0x000720ec   COMPRESSED   0x00000008   Data   RW         1503    .data               CVWL568.lib(drv_i2c_dma.o)
    0x000720f4   COMPRESSED   0x00000004   Data   RW         1532    .data               CVWL568.lib(drv_i2c_master.o)
    0x000720f8   COMPRESSED   0x00000004   Data   RW         1563    .data               CVWL568.lib(drv_i2c_slave.o)
    0x000720fc   COMPRESSED   0x000004a4   Data   RW         1588    .data               CVWL568.lib(drv_param_init.o)
    0x000725a0   COMPRESSED   0x00000004   Data   RW         1655    .data               CVWL568.lib(drv_spi_master.o)
    0x000725a4   COMPRESSED   0x00000008   Data   RW         1681    .data               CVWL568.lib(drv_swire.o)
    0x000725ac   COMPRESSED   0x00000001   Data   RW         1706    .data               CVWL568.lib(drv_sys_cfg.o)
    0x000725ad   COMPRESSED   0x00000003   PAD
    0x000725b0   COMPRESSED   0x00000050   Data   RW         1739    .data               CVWL568.lib(drv_timer.o)
    0x00072600   COMPRESSED   0x00000008   Data   RW         2085    .data               CVWL568.lib(drv_rxbr.o)
    0x00072608   COMPRESSED   0x00000004   Data   RW         2158    .data               CVWL568.lib(drv_vidc.o)
    0x0007260c   COMPRESSED   0x00000001   Data   RW         2305    .data               CVWL568.lib(drv_phy_common.o)
    0x0007260d   COMPRESSED   0x00000003   PAD
    0x00072610   COMPRESSED   0x0000000c   Data   RW         2325    .data               CVWL568.lib(drv_chip_info.o)
    0x0007261c   COMPRESSED   0x00000006   Data   RW         2362    .data               tp_EncryptCheck.lib(app_tp_enc.o)
    0x00072622   COMPRESSED   0x00000002   PAD
    0x00072624   COMPRESSED   0x00000012   Data   RW         2522    .data               CVWL568.lib(norflash.o)
    0x00072636   COMPRESSED   0x00000002   PAD
    0x00072638   COMPRESSED   0x0000000c   Data   RW         2609    .data               CVWL568.lib(drv_pwm.o)
    0x00072644   COMPRESSED   0x00000008   Data   RW         2687    .data               CVWL568.lib(drv_uart.o)
    0x0007264c   COMPRESSED   0x0000000c   Data   RW         2754    .data               CVWL568.lib(drv_wdg.o)
    0x00072658   COMPRESSED   0x00000004   Data   RW         3103    .data               mc_p.l(stdout.o)
    0x0007265c   COMPRESSED   0x00000004   Data   RW         3115    .data               mc_p.l(errno.o)
    0x00072660        -       0x00000190   Zero   RW          291    .bss                app_tp_transfer.o
    0x000727f0        -       0x0000000c   Zero   RW          429    .bss                app_tp_st_touch.o
    0x000727fc        -       0x000000c4   Zero   RW          589    .bss                CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000728c0        -       0x0000004c   Zero   RW          688    .bss                CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0007290c        -       0x000000d0   Zero   RW         1081    .bss                CVWL568.lib(hal_uart.o)
    0x000729dc        -       0x00000984   Zero   RW         1137    .bss                CVWL568.lib(hal_internal_vsync.o)
    0x00073360        -       0x0000001c   Zero   RW         1327    .bss                CVWL568.lib(drv_dma.o)
    0x0007337c        -       0x00000040   Zero   RW         1464    .bss                CVWL568.lib(drv_gpio.o)
    0x000733bc        -       0x00000140   Zero   RW         1502    .bss                CVWL568.lib(drv_i2c_dma.o)
    0x000734fc        -       0x00001030   Zero   RW         1762    .bss                CVWL568.lib(dcs_packet_fifo.o)
    0x0007452c        -       0x00000100   Zero   RW         2353    .bss                CVWL568.lib(tau_log.o)
    0x0007462c        -       0x00000020   Zero   RW         2457    .bss                CVWL568.lib(hal_spi_slave.o)
    0x0007464c   COMPRESSED   0x00000004   PAD
    0x00074650        -       0x00001000   Zero   RW          536    STACK               startup_armcm0.o


==============================================================================

Image component sizes


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Object Name

      6524        214        248       7526          0      39557   ap_demo.o
       882         66          0         40         12      10552   app_tp_st_touch.o
      1044        102          0         23        400      14196   app_tp_transfer.o
        36          6          0          0          0        553   board.o
        10          0          0          0          0       5703   main.o
       120         18        192          0       4096       2116   startup_armcm0.o

    ----------------------------------------------------------------------
      8622        406        488       7592       4508      72677   Object Totals
         0          0         48          0          0          0   (incl. Generated)
         6          0          0          3          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Member Name

       216         32          0          0       4144        252   dcs_packet_fifo.o
       272         96          0         12          0        256   drv_chip_info.o
       192         82         24         12          0        264   drv_common.o
       420         90          0          0          0       1200   drv_crgu.o
       410         28          0          0         28        796   drv_dma.o
       232         28          0          0          0        340   drv_dsc_dec.o
      1644        494          0          0          0       1336   drv_dsi_rx.o
      1528        118          0          0          0       2428   drv_dsi_tx.o
       132          0          0          0          0        256   drv_efuse.o
        10          0          0          0          0         60   drv_fls.o
       796        112          0          4         64       1236   drv_gpio.o
       600         82          0          8        320        624   drv_i2c_dma.o
       360         86          0          4          0        456   drv_i2c_master.o
       292         36          0          4          0        580   drv_i2c_slave.o
       704          6          0          0          0       1504   drv_lcdc.o
       492         28          0          0          0       1112   drv_memc.o
       112         36          8       1188          0        376   drv_param_init.o
       428         30        390          1          0        664   drv_phy_common.o
        72         10          0         12          0         76   drv_pwm.o
       112         24          0          0          0        180   drv_pwr.o
       722         84          0          8          0       1456   drv_rxbr.o
       104         24          0          4          0        188   drv_spi_master.o
       144         16          0          8          0        200   drv_swire.o
       300         64          0          1          0        628   drv_sys_cfg.o
       358         30          0         80          0        872   drv_timer.o
       698         18          0          8          0        680   drv_uart.o
       510         28          0          4          0       1452   drv_vidc.o
       168         22          0         12          0        316   drv_wdg.o
      3328        398         72          8        196       1668   hal_dsi_rx_ctrl.o
      4344        304        103          3         76       2408   hal_dsi_tx_ctrl.o
       450         48        210          0          0        752   hal_gpio.o
       212         40          0          1          0        340   hal_i2c_master.o
       696         70         32         32          0        408   hal_i2c_slave.o
      8084       1704        308         24       2436       2616   hal_internal_vsync.o
        14          0          0          0          0         68   hal_spi_master.o
       580         32          0          0         32        136   hal_spi_slave.o
        22          0          0          0          0         68   hal_swire.o
       196         32          0          0          0        408   hal_system.o
       138          6          0          0          0        208   hal_timer.o
       156         18          0          0        208        144   hal_uart.o
      1076        324          0          0        192       1980   irq_redirect .o
        48         10          0         18          0         68   norflash.o
        58          0          0          0          0        128   tau_delay.o
        60         10          0          0        256        156   tau_log.o
      1784         74       8529        287          0      18027   app_tp_for_custom_s8.o
       200         20          0          0          0         76   ceil.o
        72          6          0          0          0         76   sqrt.o
        86          0          0          0          0          0   __dczerorl2.o
         0          0          0          0          0          0   entry.o
         0          0          0          0          0          0   entry10a.o
         0          0          0          0          0          0   entry11a.o
         8          4          0          0          0          0   entry2.o
         4          0          0          0          0          0   entry5.o
         0          0          0          0          0          0   entry7b.o
         0          0          0          0          0          0   entry8b.o
         8          4          0          0          0          0   entry9a.o
        12          6          0          4          0         60   errno.o
        30          0          0          0          0          0   handlers.o
        40          0          0          0          0         72   idiv.o
        36          8          0          0          0         68   init.o
         0          0          0          0          0          0   iusefp.o
        32          0          0          0          0         68   llshl.o
        38          0          0          0          0         68   llsshr.o
        34          0          0          0          0         68   llushr.o
        36          0          0          0          0         60   memcpya.o
        36          0          0          0          0        100   memseta.o
      2298        104          0          0          0        544   printfa.o
         0          0          0          4          0          0   stdout.o
        44          0          0          0          0         72   uidiv.o
        96          0          0          0          0         84   uldiv.o
        40          2          0          0          0         68   cdcmple.o
        40          2          0          0          0         68   cdrcmple.o
        20          0          0          0          0         68   cfrcmple.o
       356          4          0          0          0        140   dadd.o
       240          6          0          0          0         84   ddiv.o
       236          0          0          0          0        216   depilogue.o
        72         10          0          0          0         72   dfixi.o
        60         10          0          0          0         68   dfixui.o
        64         10          0          0          0         68   dfixul.o
        28          4          0          0          0         68   dfltui.o
       208          6          0          0          0         88   dmul.o
       162          0          0          0          0         80   dsqrt.o
        40          0          0          0          0         60   f2d.o
       178          0          0          0          0        108   fadd.o
       124          0          0          0          0         72   fdiv.o
       130          0          0          0          0        144   fepilogue.o
        50          0          0          0          0         60   ffixi.o
        40          0          0          0          0         60   ffixui.o
        22          0          0          0          0         68   fflti.o
        14          0          0          0          0         68   ffltui.o
       122          0          0          0          0         72   fmul.o
        24          0          0          0          0         60   fscalb.o
       100         10          0          6          0       4107   app_tp_enc.o

    ----------------------------------------------------------------------
     38806       4990       9684       1768       7956      56754   Library Totals
        52          0          8         11          4          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Name

     31490       4700       1147       1456       7952      31344   CVWL568.lib
      1784         74       8529        287          0      18027   WL568_20U_HX667_TP.lib
       272         26          0          0          0        152   m_ps.l
      2838        126          0          8          0       1264   mc_p.l
      2270         54          0          0          0       1860   mf_p.l
       100         10          0          6          0       4107   tp_EncryptCheck.lib

    ----------------------------------------------------------------------
     38806       4990       9684       1768       7956      56754   Library Totals

    ----------------------------------------------------------------------

==============================================================================


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   

     47428       5396      10172       9360      12464     104947   Grand Totals
     47428       5396      10172       5200      12464     104947   ELF Image Totals (compressed)
     47428       5396      10172       5200          0          0   ROM Totals

==============================================================================

    Total RO  Size (Code + RO Data)                57600 (  56.25kB)
    Total RW  Size (RW Data + ZI Data)             21824 (  21.31kB)
    Total ROM Size (Code + RO Data + RW Data)      62800 (  61.33kB)

==============================================================================

