Component: ARM Compiler 5.06 update 6 (build 750) Tool: armlink [4d35ed]

==============================================================================

Section Cross References

    main.o(i.main) refers to board.o(i.board_Init) for board_Init
    main.o(i.main) refers to ap_demo.o(i.ap_demo) for ap_demo
    ap_demo.o(i.Gpio_swire_output) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    ap_demo.o(i.Gpio_swire_output) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.Gpio_swire_output) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    ap_demo.o(i.Gpio_swire_output) refers to tau_delay.o(i.delayUs) for delayUs
    ap_demo.o(i.PWM_OUTPUT_TEST) refers to ap_demo.o(i.test_pwm_out_adjust) for test_pwm_out_adjust
    ap_demo.o(i.PWM_OUTPUT_TEST) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.PWM_Task) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.PWM_Task) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.PWM_Task) refers to app_tp_for_custom_s8.o(.data) for Flag_blacklight_EN
    ap_demo.o(i.PWM_Task) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) for hal_dsi_rx_ctrl_get_max_ret_size
    ap_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) for hal_dsi_rx_ctrl_send_ack_cmd
    ap_demo.o(i.ap_dcs_read) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_dcs_read) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_demo) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_I2C_init) for app_tp_I2C_init
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.open_mipi_rx) for open_mipi_rx
    ap_demo.o(i.ap_demo) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_demo) refers to hal_pwm.o(i.hal_pwm_out_init) for hal_pwm_out_init
    ap_demo.o(i.ap_demo) refers to hal_pwm.o(i.hal_pwm_out_config_all) for hal_pwm_out_config_all
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.init_mipi_tx) for init_mipi_tx
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_init) for app_tp_init
    ap_demo.o(i.ap_demo) refers to hal_timer.o(i.hal_timer_init) for hal_timer_init
    ap_demo.o(i.ap_demo) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    ap_demo.o(i.ap_demo) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.init_panel) for init_panel
    ap_demo.o(i.ap_demo) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_phone_clear_reset_on) for app_tp_phone_clear_reset_on
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_transfer_screen_start) for app_tp_transfer_screen_start
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.PWM_Task) for PWM_Task
    ap_demo.o(i.ap_demo) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.app_tp_calibration_exec) for app_tp_calibration_exec
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_transfer_screen_int) for app_tp_transfer_screen_int
    ap_demo.o(i.ap_demo) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) for hal_dsi_rx_ctrl_dsc_async_handler
    ap_demo.o(i.ap_demo) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) for hal_dsi_tx_ctrl_stop
    ap_demo.o(i.ap_demo) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) for hal_dsi_tx_ctrl_deinit
    ap_demo.o(i.ap_demo) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) for hal_dsi_rx_ctrl_stop
    ap_demo.o(i.ap_demo) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) for hal_dsi_rx_ctrl_deinit
    ap_demo.o(i.ap_demo) refers to hal_swire.o(i.hal_swire_open) for hal_swire_open
    ap_demo.o(i.ap_demo) refers to hal_timer.o(i.hal_timer_stop) for hal_timer_stop
    ap_demo.o(i.ap_demo) refers to hal_system.o(i.hal_system_set_vcc) for hal_system_set_vcc
    ap_demo.o(i.ap_demo) refers to app_tp_for_custom_s8.o(.data) for tp_sleep_in
    ap_demo.o(i.ap_demo) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.soft_timer3_cb) for soft_timer3_cb
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.ap_reset_cb) for ap_reset_cb
    ap_demo.o(i.ap_get_reg_ca) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_get_reg_df) refers to memcpya.o(.text) for __aeabi_memcpy4
    ap_demo.o(i.ap_get_reg_df) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) for hal_dsi_tx_ctrl_set_ccm
    ap_demo.o(i.ap_get_reg_df) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_reset_cb) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_reset_cb) refers to hal_system.o(i.hal_system_set_pvd) for hal_system_set_pvd
    ap_demo.o(i.ap_reset_cb) refers to hal_system.o(i.hal_system_set_vcc) for hal_system_set_vcc
    ap_demo.o(i.ap_set_backlight) refers to idiv.o(.text) for __aeabi_idivmod
    ap_demo.o(i.ap_set_backlight) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_set_display_off) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_display_off) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_display_on) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) for hal_dsi_rx_ctrl_set_sw_tear_mode
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to ap_demo.o(i.Gpio_swire_output) for Gpio_swire_output
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin) for hal_dsi_tx_ctrl_panel_reset_pin
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_set_exit_sleep_mode) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_exit_sleep_mode) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_set_tp_calibration_04) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.app_tp_calibration_exec) refers to app_tp_transfer.o(i.ap_tp_calibration) for ap_tp_calibration
    ap_demo.o(i.app_tp_calibration_exec) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.app_tp_calibration_exec) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.init_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) for hal_dsi_tx_ctrl_create_handle
    ap_demo.o(i.init_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    ap_demo.o(i.init_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) for hal_dsi_tx_ctrl_set_overwrite_rgb
    ap_demo.o(i.init_mipi_tx) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin) for hal_dsi_tx_ctrl_panel_reset_pin
    ap_demo.o(i.init_panel) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.init_panel) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) for hal_dsi_tx_ctrl_enter_init_panel_mode
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) for hal_dsi_tx_ctrl_write_array_cmd
    ap_demo.o(i.init_panel) refers to tau_delay.o(i.delayUs) for delayUs
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.init_panel) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) for hal_dsi_rx_ctrl_set_hw_tear_mode
    ap_demo.o(i.init_panel) refers to ap_demo.o(i.Gpio_swire_output) for Gpio_swire_output
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) for hal_dsi_tx_ctrl_exit_init_panel_mode
    ap_demo.o(i.init_panel) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.init_panel) refers to ap_demo.o(.constdata) for .constdata
    ap_demo.o(i.init_panel) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.open_mipi_rx) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) for hal_dsi_rx_ctrl_create_handle
    ap_demo.o(i.open_mipi_rx) refers to memcpya.o(.text) for __aeabi_memcpy4
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) for hal_dsi_rx_ctrl_pre_init_pps
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) for hal_dsi_rx_ctrl_set_cus_sync_line
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) for hal_dsi_rx_ctrl_set_cus_esc_clk
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(.constdata) for .constdata
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(i.ap_dcs_read) for ap_dcs_read
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(i.pps_update_handle) for pps_update_handle
    ap_demo.o(i.pps_update_handle) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) for hal_dsi_rx_ctrl_toggle_resolution
    ap_demo.o(i.pps_update_handle) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.pps_update_handle) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.soft_timer3_cb) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    ap_demo.o(i.soft_timer3_cb) refers to app_tp_for_custom_s8.o(.data) for tp_sleep_count
    ap_demo.o(i.soft_timer3_cb) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.test_pwm_out_adjust) refers to uidiv.o(.text) for __aeabi_uidivmod
    ap_demo.o(i.test_pwm_out_adjust) refers to hal_pwm.o(i.hal_pwm_out_init) for hal_pwm_out_init
    ap_demo.o(i.test_pwm_out_adjust) refers to hal_pwm.o(i.hal_pwm_out_config_all) for hal_pwm_out_config_all
    ap_demo.o(i.test_pwm_out_adjust) refers to hal_pwm.o(i.hal_pwm_out_sync_all) for hal_pwm_out_sync_all
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_display_on) for ap_set_display_on
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_display_off) for ap_set_display_off
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_get_reg_df) for ap_get_reg_df
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_get_reg_ca) for ap_get_reg_ca
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_backlight) for ap_set_backlight
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_enter_sleep_mode) for ap_set_enter_sleep_mode
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_exit_sleep_mode) for ap_set_exit_sleep_mode
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_tp_calibration_04) for ap_set_tp_calibration_04
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to app_tp_for_custom_s8.o(.data) for .data
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to app_tp_for_custom_s8.o(.constdata) for .constdata
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to app_tp_transfer.o(i.app_tp_screen_init) for app_tp_screen_init
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to tau_log.o(i.LOG_printf) for LOG_printf
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to app_tp_for_custom_s8.o(.data) for .data
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to uidiv.o(.text) for __aeabi_uidivmod
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to app_tp_for_custom_s8.o(.data) for .data
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_1
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_2
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_3
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_4
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_5
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_6
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_7
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_point_data
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_point_back
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_coord_data
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_coord_back
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.constdata) for phone_b6_00_28_data
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.constdata) for phone_b6_00_28_back
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_transfer.o(i.S20_Start_init) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.S20_Start_init) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_ctrl_eint) for hal_gpio_ctrl_eint
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_init_eint) for hal_gpio_init_eint
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_reg_eint_cb) for hal_gpio_reg_eint_cb
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_for_custom_s8.o(.data) for screen_reg_int_data
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(i.app_tp_screen_int_callback) for app_tp_screen_int_callback
    app_tp_transfer.o(i.S20_Start_init) refers to ap_demo.o(.data) for phone_start_flag
    app_tp_transfer.o(i.ap_tp_calibration) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_transfer.o(i.ap_tp_calibration) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.ap_tp_calibration) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_transfer.o(i.ap_tp_calibration) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_I2C_init) refers to hal_i2c_slave.o(i.hal_i2c_s_init) for hal_i2c_s_init
    app_tp_transfer.o(i.app_tp_I2C_init) refers to hal_i2c_slave.o(i.hal_i2c_s_set_transfer) for hal_i2c_s_set_transfer
    app_tp_transfer.o(i.app_tp_I2C_init) refers to hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read) for hal_i2c_s_nonblocking_read
    app_tp_transfer.o(i.app_tp_I2C_init) refers to app_tp_transfer.o(i.app_tp_i2cs_callback) for app_tp_i2cs_callback
    app_tp_transfer.o(i.app_tp_I2C_init) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) for app_tp_phone_analysis_data
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(i.app_tp_s_read) for app_tp_s_read
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(i.app_tp_s_write) for app_tp_s_write
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.app_tp_init) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(i.app_tp_screen_init) for app_tp_screen_init
    app_tp_transfer.o(i.app_tp_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_master.o(i.hal_i2c_m_dma_init) for hal_i2c_m_dma_init
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_for_custom_s8.o(.data) for g_phone_output_int_pad
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_rst_pad
    app_tp_transfer.o(i.app_tp_m_read) refers to hal_i2c_master.o(i.hal_i2c_m_dma_read) for hal_i2c_m_dma_read
    app_tp_transfer.o(i.app_tp_m_transfer_complate) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.app_tp_m_write) refers to hal_i2c_master.o(i.hal_i2c_m_dma_write) for hal_i2c_m_dma_write
    app_tp_transfer.o(i.app_tp_phone_clear_reset_on) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_phone_reset_on) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_s_read) refers to hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read) for hal_i2c_s_nonblocking_read
    app_tp_transfer.o(i.app_tp_s_transfer_complate) refers to hal_i2c_slave.o(i.hal_i2c_s_write_complate) for hal_i2c_s_write_complate
    app_tp_transfer.o(i.app_tp_s_transfer_complate) refers to hal_i2c_slave.o(i.hal_i2c_s_read_complate) for hal_i2c_s_read_complate
    app_tp_transfer.o(i.app_tp_s_write) refers to hal_i2c_slave.o(i.hal_i2c_s_dma_write) for hal_i2c_s_dma_write
    app_tp_transfer.o(i.app_tp_screen_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    app_tp_transfer.o(i.app_tp_screen_init) refers to tau_delay.o(i.delayUs) for delayUs
    app_tp_transfer.o(i.app_tp_screen_init) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_transfer.o(i.app_tp_screen_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_rst_pad
    app_tp_transfer.o(i.app_tp_screen_int_callback) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to hal_spi_master.o(i.hal_spi_m_clear_rxfifo) for hal_spi_m_clear_rxfifo
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(i.S20_Start_init) for S20_Start_init
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_for_custom_s8.o(.constdata) for screen_reg_start_data_size
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to ap_demo.o(.data) for phone_start_flag
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_spi_master.o(i.hal_spi_m_clear_rxfifo) for hal_spi_m_clear_rxfifo
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_transfer_screen_const) for app_tp_transfer_screen_const
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) for app_tp_screen_analysis_int
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(.data) for screen_reg_int_data
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.app_tp_transfer_screen_start) refers to app_tp_transfer.o(i.app_tp_transfer_screen_const) for app_tp_transfer_screen_const
    app_tp_transfer.o(i.app_tp_transfer_screen_start) refers to app_tp_transfer.o(.data) for .data
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_init) for hal_system_init
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_enable_systick) for hal_system_enable_systick
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_init_console) for hal_system_init_console
    startup_armcm0.o(RESET) refers to startup_armcm0.o(STACK) for __initial_sp
    startup_armcm0.o(RESET) refers to startup_armcm0.o(.text) for Reset_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.HardFault_Handler) for HardFault_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SysTick_Handler) for SysTick_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.VIDC_IRQn_Handler) for VIDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.LCDC_IRQn_Handler) for LCDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.MIPI_RX_IRQn_Handler) for MIPI_RX_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.MIPI_TX_IRQn_Handler) for MIPI_TX_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.MEMC_IRQn_Handler) for MEMC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.VPRE_IRQn_Handler) for VPRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.FLSCTRL_IRQn_Handler) for FLSCTRL_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.DMA_IRQn_Handler) for DMA_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER0_IRQn_Handler) for TIMER0_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER1_IRQn_Handler) for TIMER1_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER2_IRQn_Handler) for TIMER2_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER3_IRQn_Handler) for TIMER3_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.WDG_IRQn_Handler) for WDG_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.UART_IRQn_Handler) for UART_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.I2C0_IRQn_Handler) for I2C0_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.I2C1_IRQn_Handler) for I2C1_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SPIS_IRQn_Handler) for SPIS_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SPIM_IRQn_Handler) for SPIM_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.ADC_IRQn_Handler) for ADC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.PWMDET_IRQn_Handler) for PWMDET_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SWIRE_IRQn_Handler) for SWIRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.AP_NRESET_IRQn_Handler) for AP_NRESET_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT0_IRQn_Handler) for EXTI_INT0_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT1_IRQn_Handler) for EXTI_INT1_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT2_IRQn_Handler) for EXTI_INT2_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT3_IRQn_Handler) for EXTI_INT3_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT4_IRQn_Handler) for EXTI_INT4_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT5_IRQn_Handler) for EXTI_INT5_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT6_IRQn_Handler) for EXTI_INT6_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT7_IRQn_Handler) for EXTI_INT7_IRQn_Handler
    startup_armcm0.o(.text) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to drv_vidc.o(i.drv_vidc_set_module_enable) for drv_vidc_set_module_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) for dcs_packet_get_fifo_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) for dcs_packet_free_fifo_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg) for drv_dsi_rx_set_ddi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_crgu.o(i.drv_crgu_set_rxbr_src) for drv_crgu_set_rxbr_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_crgu.o(i.drv_crgu_set_rxbr_div) for drv_crgu_set_rxbr_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg) for drv_dsi_rx_set_ipi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_gen_a_tear_signal) for drv_memc_gen_a_tear_signal
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size) for drv_dsi_rx_get_max_ret_size
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_rxbr_src) for drv_crgu_set_rxbr_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_rxbr_div) for drv_crgu_set_rxbr_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) for drv_dsi_rx_calc_ipi_tx_delay
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg) for drv_dsi_rx_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_dsco_src) for drv_crgu_set_dsco_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_dsco_src_div) for drv_crgu_set_dsco_src_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_dsc_core_div) for drv_crgu_set_dsc_core_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_vidc_src) for drv_crgu_set_vidc_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_fb_src) for drv_crgu_set_fb_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_fb_div) for drv_crgu_set_fb_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) for hal_dsi_rx_ctrl_init_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_rx) for hal_internal_vsync_init_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) for hal_dsi_rx_ctrl_init_dsi_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) for hal_dsi_rx_ctrl_init_rxbr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps) for drv_dsc_dec_set_u8_pps
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) for hal_dsi_rx_ctrl_init_vidc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) for hal_dsi_rx_ctrl_init_memc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_chip_info.o(i.drv_chip_rx_init_done) for drv_chip_rx_init_done
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_src) for drv_crgu_set_rxbr_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_div) for drv_crgu_set_rxbr_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dsco_src) for drv_crgu_set_dsco_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dsco_src_div) for drv_crgu_set_dsco_src_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dsc_core_div) for drv_crgu_set_dsc_core_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_fb_src) for drv_crgu_set_fb_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_fb_div) for drv_crgu_set_fb_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_vidc_src) for drv_crgu_set_vidc_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg) for drv_dsi_rx_set_ctrl_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) for drv_dsi_rx_calc_ipi_tx_delay
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg) for drv_dsi_rx_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) for drv_dsi_rx_set_up_phy
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap) for drv_dsi_rx_set_lane_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_inten) for drv_dsi_rx_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_mode) for drv_memc_set_ltpo_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_fs_en_conditions) for drv_memc_set_fs_en_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_lcdc_st_conditions) for drv_memc_set_lcdc_st_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_vidc_sync_cnt) for drv_memc_set_vidc_sync_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_double_buffer) for drv_memc_set_double_buffer
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_active_height) for drv_memc_set_active_height
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_inten) for drv_memc_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_color_format) for drv_rxbr_set_color_format
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th) for drv_rxbr_set_ltpo_drop_th
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_cfg) for drv_rxbr_set_usr_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_col) for drv_rxbr_set_usr_col
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_row) for drv_rxbr_set_usr_row
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg) for drv_rxbr_hline_rcv_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) for hal_internal_vsync_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_src_parameter) for drv_vidc_set_src_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pentile_swap) for drv_vidc_set_pentile_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_dst_parameter) for drv_vidc_set_dst_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_init_module_enable) for drv_vidc_init_module_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_rotation) for drv_vidc_set_rotation
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_init_get_scld_filter_h) for drv_param_init_get_scld_filter_h
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_init_get_scld_filter_v) for drv_param_init_get_scld_filter_v
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef0) for drv_vidc_set_scld_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef1) for drv_vidc_set_scld_hcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef0) for drv_vidc_set_scld_vcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef1) for drv_vidc_set_scld_vcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_p2r_hinitr) for drv_vidc_set_p2r_hinitr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_p2r_hinitb) for drv_vidc_set_p2r_hinitb
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_p2r_filter_init) for drv_param_p2r_filter_init
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_p2r_hcoef0) for drv_vidc_set_p2r_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_mirror) for drv_vidc_set_mirror
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pu_ctrl) for drv_vidc_set_pu_ctrl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter) for drv_dsc_dec_convert_pps_rc_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header) for drv_rxbr_set_ack_pkt_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) for hal_internal_vsync_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef0) for drv_vidc_set_scld_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef1) for drv_vidc_set_scld_hcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef0) for drv_vidc_set_scld_vcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef1) for drv_vidc_set_scld_vcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_param_init.o(i.drv_param_init_set_scld_filter) for drv_param_init_set_scld_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) for hal_internal_vsync_set_sync_line
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg) for drv_rxbr_hline_rcv0_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_dcs_direct_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode) for hal_internal_vsync_set_dcs_direct_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) refers to drv_rxbr.o(i.drv_rxbr_set_cmd_filter) for drv_rxbr_set_cmd_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format) refers to drv_vidc.o(i.drv_vidc_update_src_format) for drv_vidc_update_src_format
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format) refers to drv_vidc.o(i.drv_vidc_set_pentile_swap) for drv_vidc_set_pentile_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dflti.o(.text) for __aeabi_i2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dmul.o(.text) for __aeabi_dmul
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to ddiv.o(.text) for __aeabi_ddiv
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_te_waveform) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_te_waveform) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_dsi_rx.o(i.drv_dsi_rx_power_up) for drv_dsi_rx_power_up
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg) for drv_rxbr_hline_rcv0_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) for hal_internal_sync_input_resolution_change
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fscalb.o(.text) for __ARM_scalbnf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fflti.o(.text) for __aeabi_i2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to ffixi.o(.text) for __aeabi_f2iz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk) for drv_dsi_tx_set_video_chunk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing) for drv_dsi_tx_set_video_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to drv_phy_common.o(i.drv_phy_get_para) for drv_phy_get_para
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to ffixui.o(.text) for __aeabi_f2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_ulps_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) for drv_dsi_tx_phy_ulps_enter
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_ulps_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) for drv_dsi_tx_phy_ulps_exit
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) for hal_dsi_tx_ctrl_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_tx) for hal_internal_vsync_init_tx
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) for hal_dsi_tx_count_lane_rate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) for hal_dsi_tx_init_phy_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_phy_test_setup) for hal_dsi_tx_phy_test_setup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) for hal_lcdc_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) for hal_lcdc_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) for hal_dsi_tx_init_dpi_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) for hal_dsi_tx_init_data_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) for hal_dsi_tx_init_remains
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt) for hal_dsi_tx_init_interrupt
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready) for drv_dsi_tx_phy_status_ready
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_bta) for drv_dsi_tx_set_bta
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload) for drv_dsi_tx_command_get_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) refers to drv_param_init.o(i.drv_param_init_set_ccm) for drv_param_init_set_ccm
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness) refers to drv_lcdc.o(i.drv_lcdc_config_endianness) for drv_lcdc_config_endianness
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_lp_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd) for drv_dsi_tx_video_mode_set_lp_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb) for drv_lcdc_config_overwrite_rgb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp) refers to drv_lcdc.o(i.drv_lcdc_config_partial_display_enable) for drv_lcdc_config_partial_display_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area) refers to drv_lcdc.o(i.drv_lcdc_config_partial_display_area) for drv_lcdc_config_partial_display_area
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_vpg) for drv_dsi_tx_set_vpg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_enable_shadow_reg) for drv_lcdc_enable_shadow_reg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_set_video_hw_mode) for drv_lcdc_set_video_hw_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_start) for drv_lcdc_start
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_lcdc.o(i.drv_lcdc_start) for drv_lcdc_start
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size) for drv_dsi_tx_edpi_cmd_size
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) for hal_dsi_tx_init_video_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode) for drv_dsi_tx_dpi_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity) for drv_dsi_tx_dpi_polarity
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time) for drv_dsi_tx_dpi_lpcmd_time
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_int) for drv_dsi_tx_config_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode) for drv_dsi_tx_phy_lane_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg) for drv_dsi_tx_phy_time_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_response_mode) for drv_dsi_tx_response_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div) for drv_dsi_tx_set_time_out_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg) for drv_dsi_tx_timeout_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp) for drv_dsi_tx_phy_clock_lane_auto_lp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg) for drv_dsi_tx_video_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack) for drv_dsi_tx_set_bta_ack
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd) for drv_dsi_tx_video_mode_set_lp_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_disable_hact_cmd) for drv_dsi_tx_video_mode_disable_hact_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) for hal_dsi_tx_calc_video_chunks
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_phy_test_get_data) refers to hal_dsi_tx_ctrl.o(.constdata) for .constdata
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_phy_test_setup) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_get_para) for drv_phy_get_para
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_phy_test_setup) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_phy_test_get_data) for hal_dsi_tx_phy_test_get_data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_enter) for drv_tx_phy_test_enter
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_phy_test_setup) refers to drv_crgu.o(i.drv_crgu_set_mipi_ref_src) for drv_crgu_set_mipi_ref_src
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_phy_test_setup) refers to drv_crgu.o(i.drv_crgu_set_mipi_cfg_src) for drv_crgu_set_mipi_cfg_src
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_clear) for drv_tx_phy_test_clear
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) for drv_tx_phy_test_write_1_byte
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte) for drv_tx_phy_test_write_2_byte
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_code) for drv_tx_phy_test_write_code
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_exit) for drv_tx_phy_test_exit
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_header) for drv_dsi_tx_command_header
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) refers to drv_param_init.o(i.drv_param_init_get_ccm) for drv_param_init_get_ccm
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) refers to drv_lcdc.o(i.drv_lcdc_config_ccm) for drv_lcdc_config_ccm
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_disp_mode) for drv_lcdc_config_disp_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_edpi_mode) for drv_lcdc_config_edpi_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_endianness) for drv_lcdc_config_endianness
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_thresh) for drv_lcdc_config_thresh
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_dpi_polarity) for drv_lcdc_config_dpi_polarity
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_src_parameter) for drv_lcdc_config_src_parameter
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area) for hal_dsi_tx_ctrl_set_partial_disp_area
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp) for hal_dsi_tx_ctrl_set_partial_disp
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_lcdc.o(i.drv_lcdc_config_scale_up_step) for drv_lcdc_config_scale_up_step
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_lcdc.o(i.drv_lcdc_config_scale_up_coef) for drv_lcdc_config_scale_up_coef
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) for hal_lcdc_config_upscaler
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) for hal_lcdc_config_ccm
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile) for hal_lcdc_config_rgb_to_pentile
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) for hal_lcdc_config_remains
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) for hal_lcdc_init_interrupt
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dpi_pre_div) for drv_crgu_set_dpi_pre_div
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dpi_pre_src) for drv_crgu_set_dpi_pre_src
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dpi_mux_src) for drv_crgu_set_dpi_mux_src
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_lcdc.o(i.drv_lcdc_config_dpi_timing) for drv_lcdc_config_dpi_timing
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_lcdc_div) for drv_crgu_set_lcdc_div
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_lcdc_src) for drv_crgu_set_lcdc_src
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to drv_lcdc.o(i.drv_lcdc_ctrl_flow) for drv_lcdc_ctrl_flow
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to drv_lcdc.o(i.drv_lcdc_config_int) for drv_lcdc_config_int
    hal_gpio.o(i.hal_gpio_ctrl_eint) refers to drv_gpio.o(i.drv_gpio_set_int) for drv_gpio_set_int
    hal_gpio.o(i.hal_gpio_ctrl_eint) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_get_input_data) refers to drv_gpio.o(i.drv_gpio_get_input_data) for drv_gpio_get_input_data
    hal_gpio.o(i.hal_gpio_get_int_type) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to drv_gpio.o(i.drv_gpio_get_pull_state) for drv_gpio_get_pull_state
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_eint) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group) for drv_sys_cfg_sel_gpio_group
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig) for drv_sys_cfg_sel_int_trig
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_init_eint) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_input) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_input) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_input) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_init_output) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_reg_eint_cb) refers to drv_gpio.o(i.drv_gpio_register_callback) for drv_gpio_register_callback
    hal_gpio.o(i.hal_gpio_reg_eint_cb) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_gpio.o(i.drv_gpio_register_ap_reset_callback) for drv_gpio_register_ap_reset_callback
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) for drv_sys_cfg_sel_ap_rst_trig
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to drv_gpio.o(i.drv_gpio_set_driving_strength) for drv_gpio_set_driving_strength
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode3) for drv_gpio_set_mode3
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode2) for drv_gpio_set_mode2
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode1) for drv_gpio_set_mode1
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode0) for drv_gpio_set_mode0
    hal_gpio.o(i.hal_gpio_set_mode) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_output_data) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to drv_gpio.o(i.drv_gpio_set_pull_state) for drv_gpio_set_pull_state
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to drv_gpio.o(i.drv_gpio_set_schmitt_trigger) for drv_gpio_set_schmitt_trigger
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to drv_gpio.o(i.drv_gpio_set_slew_rate) for drv_gpio_set_slew_rate
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to hal_gpio.o(.constdata) for .constdata
    hal_pwm.o(i.hal_pwm_in_clear_int) refers to drv_pwm.o(i.drv_pwm_in_clear_pwm_int_all) for drv_pwm_in_clear_pwm_int_all
    hal_pwm.o(i.hal_pwm_in_config_int) refers to drv_pwm.o(i.drv_pwm_in_set_pwm_int) for drv_pwm_in_set_pwm_int
    hal_pwm.o(i.hal_pwm_in_ctrl_int) refers to drv_pwm.o(i.drv_pwm_in_set_sys_int) for drv_pwm_in_set_sys_int
    hal_pwm.o(i.hal_pwm_in_deinit) refers to drv_pwm.o(i.drv_pwm_in_enable) for drv_pwm_in_enable
    hal_pwm.o(i.hal_pwm_in_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_pwm.o(i.hal_pwm_in_get_current_count) refers to drv_pwm.o(i.drv_pwm_in_get_current_count) for drv_pwm_in_get_current_count
    hal_pwm.o(i.hal_pwm_in_get_high_period) refers to drv_pwm.o(i.drv_pwm_in_get_high_period) for drv_pwm_in_get_high_period
    hal_pwm.o(i.hal_pwm_in_get_high_period) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_pwm.o(i.hal_pwm_in_get_high_period) refers to drv_common.o(.data) for g_system_clock
    hal_pwm.o(i.hal_pwm_in_get_low_period) refers to drv_pwm.o(i.drv_pwm_in_get_low_period) for drv_pwm_in_get_low_period
    hal_pwm.o(i.hal_pwm_in_get_low_period) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_pwm.o(i.hal_pwm_in_get_low_period) refers to drv_common.o(.data) for g_system_clock
    hal_pwm.o(i.hal_pwm_in_get_total_period) refers to drv_pwm.o(i.drv_pwm_in_get_counter_period) for drv_pwm_in_get_counter_period
    hal_pwm.o(i.hal_pwm_in_get_total_period) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_pwm.o(i.hal_pwm_in_get_total_period) refers to drv_common.o(.data) for g_system_clock
    hal_pwm.o(i.hal_pwm_in_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_pwm.o(i.hal_pwm_in_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_pwm.o(i.hal_pwm_in_init) refers to drv_pwm.o(i.drv_pwm_in_enable) for drv_pwm_in_enable
    hal_pwm.o(i.hal_pwm_in_register_callback) refers to drv_pwm.o(i.drv_pwm_in_register_callback) for drv_pwm_in_register_callback
    hal_pwm.o(i.hal_pwm_in_set_int) refers to drv_pwm.o(i.drv_pwm_in_set_pwm_int) for drv_pwm_in_set_pwm_int
    hal_pwm.o(i.hal_pwm_out_config_all) refers to drv_pwm.o(i.drv_pwm_out_enable) for drv_pwm_out_enable
    hal_pwm.o(i.hal_pwm_out_config_all) refers to drv_pwm.o(i.drv_pwm_out_set_control) for drv_pwm_out_set_control
    hal_pwm.o(i.hal_pwm_out_config_all) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_pwm.o(i.hal_pwm_out_config_all) refers to drv_pwm.o(i.drv_pwm_out_set_threshold) for drv_pwm_out_set_threshold
    hal_pwm.o(i.hal_pwm_out_config_all) refers to drv_pwm.o(i.drv_pwm_out_set_period) for drv_pwm_out_set_period
    hal_pwm.o(i.hal_pwm_out_config_all) refers to drv_common.o(.data) for g_system_clock
    hal_pwm.o(i.hal_pwm_out_deinit) refers to drv_pwm.o(i.drv_pwm_out_enable) for drv_pwm_out_enable
    hal_pwm.o(i.hal_pwm_out_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_pwm.o(i.hal_pwm_out_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_pwm.o(i.hal_pwm_out_pause) refers to drv_pwm.o(i.drv_pwm_out_pause) for drv_pwm_out_pause
    hal_pwm.o(i.hal_pwm_out_sel_io) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_pwm.o(i.hal_pwm_out_sync_all) refers to drv_pwm.o(i.drv_pwm_out_set_sync_mode) for drv_pwm_out_set_sync_mode
    hal_pwm.o(i.hal_pwm_out_sync_all) refers to drv_pwm.o(i.drv_pwm_out_set_control) for drv_pwm_out_set_control
    hal_pwm.o(i.hal_pwm_out_sync_all) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_pwm.o(i.hal_pwm_out_sync_all) refers to drv_pwm.o(i.drv_pwm_out_set_threshold) for drv_pwm_out_set_threshold
    hal_pwm.o(i.hal_pwm_out_sync_all) refers to drv_pwm.o(i.drv_pwm_out_set_period) for drv_pwm_out_set_period
    hal_pwm.o(i.hal_pwm_out_sync_all) refers to drv_pwm.o(i.drv_pwm_out_get_sync_flag) for drv_pwm_out_get_sync_flag
    hal_pwm.o(i.hal_pwm_out_sync_all) refers to tau_delay.o(i.delayUs) for delayUs
    hal_pwm.o(i.hal_pwm_out_sync_all) refers to drv_common.o(.data) for g_system_clock
    hal_pwm.o(i.hal_pwm_out_sync_ctl) refers to drv_pwm.o(i.drv_pwm_out_set_sync_mode) for drv_pwm_out_set_sync_mode
    hal_pwm.o(i.hal_pwm_out_sync_ctl) refers to drv_pwm.o(i.drv_pwm_out_set_control) for drv_pwm_out_set_control
    hal_pwm.o(i.hal_pwm_out_sync_pause) refers to drv_pwm.o(i.drv_pwm_out_set_sync_mode) for drv_pwm_out_set_sync_mode
    hal_pwm.o(i.hal_pwm_out_sync_pause) refers to drv_pwm.o(i.drv_pwm_out_pause) for drv_pwm_out_pause
    hal_pwm.o(i.hal_pwm_out_sync_period) refers to drv_pwm.o(i.drv_pwm_out_set_sync_mode) for drv_pwm_out_set_sync_mode
    hal_pwm.o(i.hal_pwm_out_sync_period) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_pwm.o(i.hal_pwm_out_sync_period) refers to drv_pwm.o(i.drv_pwm_out_set_period) for drv_pwm_out_set_period
    hal_pwm.o(i.hal_pwm_out_sync_period) refers to drv_common.o(.data) for g_system_clock
    hal_pwm.o(i.hal_pwm_out_sync_thr) refers to drv_pwm.o(i.drv_pwm_out_set_sync_mode) for drv_pwm_out_set_sync_mode
    hal_pwm.o(i.hal_pwm_out_sync_thr) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_pwm.o(i.hal_pwm_out_sync_thr) refers to drv_pwm.o(i.drv_pwm_out_set_threshold) for drv_pwm_out_set_threshold
    hal_pwm.o(i.hal_pwm_out_sync_thr) refers to drv_common.o(.data) for g_system_clock
    hal_swire.o(i.hal_swire_deinit) refers to drv_swire.o(i.drv_swire_enable) for drv_swire_enable
    hal_swire.o(i.hal_swire_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_swire.o(i.hal_swire_init) refers to drv_crgu.o(i.drv_crgu_set_swire_div) for drv_crgu_set_swire_div
    hal_swire.o(i.hal_swire_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_swire.o(i.hal_swire_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_swire.o(i.hal_swire_init) refers to drv_swire.o(i.drv_swire_enable) for drv_swire_enable
    hal_swire.o(i.hal_swire_open) refers to drv_swire.o(i.drv_swire_set_power_down) for drv_swire_set_power_down
    hal_swire.o(i.hal_swire_register_callback) refers to drv_swire.o(i.drv_swire_register_callback) for drv_swire_register_callback
    hal_swire.o(i.hal_swire_start) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    hal_swire.o(i.hal_swire_start) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_swire.o(i.hal_swire_start) refers to drv_swire.o(i.drv_swire_set_bit_time) for drv_swire_set_bit_time
    hal_swire.o(i.hal_swire_start) refers to drv_swire.o(i.drv_swire_set_pulse_count) for drv_swire_set_pulse_count
    hal_swire.o(i.hal_swire_start) refers to drv_common.o(.data) for g_system_clock
    hal_system.o(i.hal_system_deep_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode) for drv_pwr_enter_deep_sleep_mode
    hal_system.o(i.hal_system_disable_systick) refers to drv_common.o(i.drv_common_disable_systick) for drv_common_disable_systick
    hal_system.o(i.hal_system_enable_systick) refers to drv_common.o(i.drv_common_enable_systick) for drv_common_enable_systick
    hal_system.o(i.hal_system_flash_read) refers to norflash.o(i.norflash_init) for norflash_init
    hal_system.o(i.hal_system_flash_read) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    hal_system.o(i.hal_system_flash_read) refers to norflash.o(i.norflash_read) for norflash_read
    hal_system.o(i.hal_system_flash_read) refers to drv_fls.o(i.fls_de_init) for fls_de_init
    hal_system.o(i.hal_system_flash_read) refers to hal_system.o(i.cvt_check_cgf_is_valid) for cvt_check_cgf_is_valid
    hal_system.o(i.hal_system_flash_write) refers to norflash.o(i.norflash_init) for norflash_init
    hal_system.o(i.hal_system_flash_write) refers to hal_system.o(i.cvt_cfg_packet) for cvt_cfg_packet
    hal_system.o(i.hal_system_flash_write) refers to norflash.o(i.norflash_erase_block) for norflash_erase_block
    hal_system.o(i.hal_system_flash_write) refers to norflash.o(i.norflash_write) for norflash_write
    hal_system.o(i.hal_system_flash_write) refers to drv_fls.o(i.fls_de_init) for fls_de_init
    hal_system.o(i.hal_system_get_tick) refers to drv_common.o(i.drv_common_get_tick) for drv_common_get_tick
    hal_system.o(i.hal_system_idle_mode) refers to drv_common.o(i.drv_common_idle_mode) for drv_common_idle_mode
    hal_system.o(i.hal_system_init) refers to drv_pwr.o(i.drv_pwr_set_system_clk_src) for drv_pwr_set_system_clk_src
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_set_ahb_src) for drv_crgu_set_ahb_src
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_set_ahb_pre_div) for drv_crgu_set_ahb_pre_div
    hal_system.o(i.hal_system_init) refers to irq_redirect .o(i.handle_init) for handle_init
    hal_system.o(i.hal_system_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int) for drv_sys_cfg_clear_all_int
    hal_system.o(i.hal_system_init) refers to drv_common.o(i.drv_common_system_init) for drv_common_system_init
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_clear_all_reset_flags) for drv_crgu_clear_all_reset_flags
    hal_system.o(i.hal_system_init) refers to drv_pwr.o(i.drv_pwr_set_pvd_mode) for drv_pwr_set_pvd_mode
    hal_system.o(i.hal_system_init) refers to drv_common.o(.data) for g_system_clock
    hal_system.o(i.hal_system_init_console) refers to hal_uart.o(i.hal_uart_init) for hal_uart_init
    hal_system.o(i.hal_system_register_systick_cb) refers to drv_common.o(i.drv_common_systick_register_cb) for drv_common_systick_register_cb
    hal_system.o(i.hal_system_set_pvd) refers to drv_pwr.o(i.drv_pwr_set_pvd_mode) for drv_pwr_set_pvd_mode
    hal_system.o(i.hal_system_set_vcc) refers to drv_pwr.o(i.drv_pwr_set_cp_mode) for drv_pwr_set_cp_mode
    hal_system.o(i.hal_system_share_flash_mode) refers to drv_fls.o(i.drv_fls_gpio_connect) for drv_fls_gpio_connect
    hal_system.o(i.hal_system_share_flash_mode) refers to drv_fls.o(i.drv_fls_gpio_disconnect) for drv_fls_gpio_disconnect
    hal_system.o(i.hal_system_sleep_mode) refers to drv_crgu.o(i.drv_crgu_config_clocks) for drv_crgu_config_clocks
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_timer.o(i.hal_timer_get_status) refers to drv_timer.o(i.drv_timer_get_current_count) for drv_timer_get_current_count
    hal_timer.o(i.hal_timer_get_status) refers to drv_timer.o(i.drv_timer_get_match) for drv_timer_get_match
    hal_timer.o(i.hal_timer_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_timer.o(i.hal_timer_init) refers to drv_timer.o(i.drv_timer_set_prescaler) for drv_timer_set_prescaler
    hal_timer.o(i.hal_timer_init) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_get_prescaler) for drv_timer_get_prescaler
    hal_timer.o(i.hal_timer_start) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_match) for drv_timer_set_match
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_current_count) for drv_timer_set_current_count
    hal_timer.o(i.hal_timer_start) refers to drv_common.o(.data) for g_system_clock
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_match) for drv_timer_set_match
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_current_count) for drv_timer_set_current_count
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_master.o(i.drv_i2c_master_init) for drv_i2c_master_init
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_master.o(i.drv_i2c_m_set_callback) for drv_i2c_m_set_callback
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_master.o(i.drv_i2c_m_enable_intr) for drv_i2c_m_enable_intr
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_dma.o(i.drv_i2c_dma_init) for drv_i2c_dma_init
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_dma.o(i.drv_i2c_enable_rx_dma) for drv_i2c_enable_rx_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_dma.o(i.drv_i2c_enable_tx_dma) for drv_i2c_enable_tx_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to hal_i2c_master.o(i.hal_i2c_master_irq_callback) for hal_i2c_master_irq_callback
    hal_i2c_master.o(i.hal_i2c_m_dma_read) refers to drv_i2c_dma.o(i.drv_i2c_master_read_dma) for drv_i2c_master_read_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_read) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_master.o(i.hal_i2c_m_dma_write) refers to drv_i2c_dma.o(i.drv_i2c_master_write_dma) for drv_i2c_master_write_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_write) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_master.o(i.hal_i2c_m_set_high_impedance) refers to drv_i2c_master.o(i.drv_i2c_m_enable) for drv_i2c_m_enable
    hal_i2c_master.o(i.hal_i2c_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_master.o(i.hal_i2c_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_i2c_master.o(i.hal_i2c_m_transfer_complate) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_master.o(i.hal_i2c_master_irq_callback) refers to drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit) for drv_i2c_m_clear_it_pending_bit
    hal_i2c_master.o(i.hal_i2c_master_irq_callback) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to drv_i2c_dma.o(i.drv_i2c_slave_write_dma) for drv_i2c_slave_write_dma
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_get_tx_byte_num) refers to drv_i2c_slave.o(i.drv_i2c_s_get_tx_byte_num) for drv_i2c_s_get_tx_byte_num
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c_slave_init) for drv_i2c_slave_init
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c_s_set_callback) for drv_i2c_s_set_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c_s_enable_intr) for drv_i2c_s_enable_intr
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_dma.o(i.drv_i2c_dma_init) for drv_i2c_dma_init
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) for drv_i2c_set_dma_irq_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_dma.o(i.drv_i2c_enable_tx_dma) for drv_i2c_enable_tx_dma
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) for hal_i2c_slave_irq_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback) for hal_i2c_s_dma_user_callback
    hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_complate) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_complate_clear) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_data) refers to drv_i2c_slave.o(i.drv_i2c_s_read_data) for drv_i2c_s_read_data
    hal_i2c_slave.o(i.hal_i2c_s_rxfifo_notempty) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    hal_i2c_slave.o(i.hal_i2c_s_set_dma_tx_cycle) refers to drv_dma.o(i.drv_dma_enable_cycle) for drv_dma_enable_cycle
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to drv_i2c_slave.o(i.drv_i2c_s_enable) for drv_i2c_s_enable
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_i2c_slave.o(i.hal_i2c_s_set_transfer) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_write_complate) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_write_data) refers to drv_i2c_slave.o(i.drv_i2c_s_write_data) for drv_i2c_s_write_data
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit) for drv_i2c_s_clear_it_pending_bit
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(i.drv_i2c_s_write_data) for drv_i2c_s_write_data
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(.data) for tx_byte_num
    hal_spi_master.o(i.hal_spi_m_callback) refers to drv_spi_dma.o(i.drv_spi_abort_dma) for drv_spi_abort_dma
    hal_spi_master.o(i.hal_spi_m_callback) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_clear_rxfifo) refers to drv_spi_master.o(i.drv_spi_m_read_data) for drv_spi_m_read_data
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to hal_spi_master.o(i.hal_spi_m_gpio_init) for hal_spi_m_gpio_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_master.o(i.drv_spi_master_init) for drv_spi_master_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_dma_init) for drv_spi_dma_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_dma_ch6_init) for drv_spi_dma_ch6_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) for drv_spi_set_dma_irq_callback
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) for drv_spi_set_dma_ch6_irq_callback
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req) for drv_sys_cfg_set_dma_rx_req
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_master.o(i.drv_spi_m_enable_rx_dma) for drv_spi_m_enable_rx_dma
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to hal_spi_master.o(i.hal_spi_m_callback) for hal_spi_m_callback
    hal_spi_master.o(i.hal_spi_m_dma_read) refers to drv_spi_dma.o(i.drv_spim_dma_read) for drv_spim_dma_read
    hal_spi_master.o(i.hal_spi_m_dma_read) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_dma_write) refers to drv_spi_dma.o(i.drv_spim_dma_write) for drv_spim_dma_write
    hal_spi_master.o(i.hal_spi_m_dma_write) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_get_transfer_complate) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_gpio_init) refers to drv_spi_master.o(i.drv_spi_m_gpio_init) for drv_spi_m_gpio_init
    hal_spi_master.o(i.hal_spi_m_read_rxfifo) refers to drv_spi_master.o(i.drv_spi_m_read_data) for drv_spi_m_read_data
    hal_spi_master.o(i.hal_spi_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_spi_master.o(i.hal_spi_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    hal_spi_master.o(i.hal_spi_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    tau_delay.o(i.delayMs) refers to tau_delay.o(i.delayUs) for delayUs
    tau_log.o(i.LOG_printf) refers to printfa.o(i.__0vsprintf) for vsprintf
    tau_log.o(i.LOG_printf) refers to printfa.o(i.__0printf) for __2printf
    tau_log.o(i.LOG_printf) refers to tau_log.o(.bss) for .bss
    tau_log.o(i.fgetc) refers to hal_uart.o(i.hal_uart_receive_blocking) for hal_uart_receive_blocking
    tau_log.o(i.fputc) refers to hal_uart.o(i.hal_uart_transmit_blocking) for hal_uart_transmit_blocking
    hal_uart.o(i.hal_uart_deinit) refers to drv_dma.o(i.drv_dma_deinit) for drv_dma_deinit
    hal_uart.o(i.hal_uart_deinit) refers to drv_uart.o(i.UART_Deinit) for UART_Deinit
    hal_uart.o(i.hal_uart_dmacallback) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_uart.o(i.hal_uart_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_uart.o(i.hal_uart_init) refers to drv_uart.o(i.UART_init) for UART_init
    hal_uart.o(i.hal_uart_init) refers to drv_common.o(.data) for g_system_clock
    hal_uart.o(i.hal_uart_init) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_receive_blocking) refers to drv_uart.o(i.UART_ReadBlocking) for UART_ReadBlocking
    hal_uart.o(i.hal_uart_receive_dma) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    hal_uart.o(i.hal_uart_receive_dma) refers to drv_uart_dma.o(i.UART_TransferCreateHandleDMA) for UART_TransferCreateHandleDMA
    hal_uart.o(i.hal_uart_receive_dma) refers to drv_uart_dma.o(i.UART_TransferReceiveDMA) for UART_TransferReceiveDMA
    hal_uart.o(i.hal_uart_receive_dma) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_receive_dma) refers to hal_uart.o(i.hal_uart_dmacallback) for hal_uart_dmacallback
    hal_uart.o(i.hal_uart_transmit_blocking) refers to drv_uart.o(i.UART_WriteBlocking) for UART_WriteBlocking
    hal_uart.o(i.hal_uart_transmit_dma) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    hal_uart.o(i.hal_uart_transmit_dma) refers to drv_uart_dma.o(i.UART_TransferCreateHandleDMA) for UART_TransferCreateHandleDMA
    hal_uart.o(i.hal_uart_transmit_dma) refers to drv_uart_dma.o(i.UART_TransferSendDMA) for UART_TransferSendDMA
    hal_uart.o(i.hal_uart_transmit_dma) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_transmit_dma) refers to hal_uart.o(i.hal_uart_dmacallback) for hal_uart_dmacallback
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to hal_internal_vsync.o(i.soft_gen_te) for soft_gen_te
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_param_init.o(i.drv_param_init_get_ccm) for drv_param_init_get_ccm
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_lcdc.o(i.drv_lcdc_config_ccm) for drv_lcdc_config_ccm
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to hal_internal_vsync.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.dcs_sw_filter) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_iniernal_vsync_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.hal_iniernal_vsync_deinit) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_mode) for drv_memc_set_ltpo_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_double_buffer) for drv_memc_set_double_buffer
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_active_height) for drv_memc_set_active_height
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_inten) for drv_memc_set_inten
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) for hal_dsi_rx_ctrl_gen_a_tear_signal
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_delay.o(i.delayUs) for delayUs
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.hal_internal_init_memc) for hal_internal_init_memc
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_chip_info.o(i.drv_chip_rx_info_check) for drv_chip_rx_info_check
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_rxbr.o(i.drv_rxbr_register_irq0_callback) for drv_rxbr_register_irq0_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_rxbr.o(i.drv_rxbr_register_irq1_callback) for drv_rxbr_register_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_vidc.o(i.drv_vidc_register_callback) for drv_vidc_register_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_init) for dcs_packet_fifo_init
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.rxbr_irq0_callback) for rxbr_irq0_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.rxbr_irq1_callback) for rxbr_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.vidc_callback) for vidc_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) refers to drv_rxbr.o(i.drv_rxbr_set_cmd_filter) for drv_rxbr_set_cmd_filter
    hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) for hal_internal_vsync_set_auto_hw_filter
    hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(i.vsync_set_te_mode) for vsync_set_te_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.vsync_set_te_mode) for vsync_set_te_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(i.dcs_sw_filter) for dcs_sw_filter
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) for dcs_packet_fifo_alloc
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) for hal_dsi_rx_ctrl_dsc_async_handler
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_rxbr.o(i.drv_rxbr_get_col_addr) for drv_rxbr_get_col_addr
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_rxbr.o(i.drv_rxbr_get_page_addr) for drv_rxbr_get_page_addr
    hal_internal_vsync.o(i.rx_partial_update) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_dsc_dec.o(i.drv_dsc_dec_get_nslc) for drv_dsc_dec_get_nslc
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_crgu.o(i.drv_crgu_set_dsco_src) for drv_crgu_set_dsco_src
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_crgu.o(i.drv_crgu_set_dsco_src_div) for drv_crgu_set_dsco_src_div
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_crgu.o(i.drv_crgu_set_dsc_core_div) for drv_crgu_set_dsc_core_div
    hal_internal_vsync.o(i.rx_partial_update) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(i.rx_get_dcs_packet_data) for rx_get_dcs_packet_data
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(i.rx_receive_pps) for rx_receive_pps
    hal_internal_vsync.o(i.rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_receive_pps) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.rx_receive_pps) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rx_receive_pps) refers to hal_internal_vsync.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter) for drv_dsc_dec_convert_pps_rc_parameter
    hal_internal_vsync.o(i.rx_receive_pps) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps) for drv_dsc_dec_set_u8_pps
    hal_internal_vsync.o(i.rx_receive_pps) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.rx_receive_pps) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.rx_receive_packet) for rx_receive_packet
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_int_source) for drv_rxbr_get_int_source
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.rx_partial_update) for rx_partial_update
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_int_source) for drv_rxbr_get_int_source
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.vpre_err_reset) for vpre_err_reset
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_memc.o(i.drv_memc_set_double_buffer_reverse) for drv_memc_set_double_buffer_reverse
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_get_irq_status) for drv_vidc_get_irq_status
    hal_internal_vsync.o(i.vidc_callback) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_clear_irq) for drv_vidc_clear_irq
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_internal_vsync.o(i.vidc_callback) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps) for drv_dsc_dec_set_u8_pps
    hal_internal_vsync.o(i.vpre_err_reset) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to drv_lcdc.o(i.drv_lcdc_ctrl_flow) for drv_lcdc_ctrl_flow
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(.data) refers to hal_internal_vsync.o(.bss) for sg_te_info
    norflash.o(i.app_fls_ctrl_Handler) refers to drv_fls.o(i.fls_clr_interrupt_flag) for fls_clr_interrupt_flag
    norflash.o(i.app_fls_ctrl_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    norflash.o(i.app_fls_ctrl_Handler) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_best_cfg_init) refers to drv_fls.o(i.fls_spi_init) for fls_spi_init
    norflash.o(i.norflash_best_cfg_init) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_check_id) refers to norflash.o(i.norflash_read_id) for norflash_read_id
    norflash.o(i.norflash_check_id) refers to tau_delay.o(i.delayUs) for delayUs
    norflash.o(i.norflash_check_id) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dma_callback) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dma_read) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_transfer_create_handle_dma) for fls_transfer_create_handle_dma
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_dma_read_prepare) for fls_dma_read_prepare
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_transfer_dma) for fls_transfer_dma
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    norflash.o(i.norflash_dma_read) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dma_read) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_dma_read) refers to norflash.o(i.norflash_dma_callback) for norflash_dma_callback
    norflash.o(i.norflash_dma_write) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_transfer_create_handle_dma) for fls_transfer_create_handle_dma
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_switch_fls_spi) for norflash_switch_fls_spi
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_dma_write_prepare) for fls_dma_write_prepare
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_transfer_dma) for fls_transfer_dma
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    norflash.o(i.norflash_dma_write) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_dma_write) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_dma_callback) for norflash_dma_callback
    norflash.o(i.norflash_dma_write) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dual_read) refers to drv_fls.o(i.fls_ddat_enable) for fls_ddat_enable
    norflash.o(i.norflash_dual_read) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_dual_read) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_switch_fls_spi) for norflash_switch_fls_spi
    norflash.o(i.norflash_dual_write) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_dual_write) refers to drv_fls.o(i.fls_ddat_enable) for fls_ddat_enable
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_en4b) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_read_config_reg) for norflash_read_config_reg
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_en_quad) refers to norflash.o(i.norflash_en_quad_check) for norflash_en_quad_check
    norflash.o(i.norflash_en_quad) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_en_quad) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_en_quad) refers to drv_fls.o(i.fls_busy_pending) for fls_busy_pending
    norflash.o(i.norflash_en_quad) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(i.norflash_get_dual_hstatus) for norflash_get_dual_hstatus
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(i.norflash_get_hstatus) for norflash_get_hstatus
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_erase_block) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_erase_block) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_erase_block) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_erase_block) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_erase_chip) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_erase_chip) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_erase_chip) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_erase_sector) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_erase_sector) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_erase_sector) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_erase_sector) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_ex4b) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_read_config_reg) for norflash_read_config_reg
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_exit_quad) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_exit_quad) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_exit_quad) refers to norflash.o(i.norflash_en_quad_check) for norflash_en_quad_check
    norflash.o(i.norflash_exit_quad) refers to drv_fls.o(i.fls_busy_pending) for fls_busy_pending
    norflash.o(i.norflash_exit_quad) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_get_dual_hstatus) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_get_dual_hstatus) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_get_dual_hstatus) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_get_hstatus) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_get_hstatus) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_get_hstatus) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_get_status) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_get_status) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_get_status) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_get_default_spi_config) for fls_get_default_spi_config
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_get_default_fls_config) for fls_get_default_fls_config
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_get_default_tuning) for fls_get_default_tuning
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_init) for fls_init
    norflash.o(i.norflash_init) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_init) refers to drv_fls.o(.data) for g_fls_tuning
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_qdat_enable) for fls_qdat_enable
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_qadr_enable) for fls_qadr_enable
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_qcmd_enable) for fls_qcmd_enable
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_switch_fls_spi) for norflash_switch_fls_spi
    norflash.o(i.norflash_quad_write) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_quad_write) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_read) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_read_config_reg) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_read_id) refers to drv_fls.o(i.fls_read_cmd) for fls_read_cmd
    norflash.o(i.norflash_set_best_cfg) refers to memseta.o(.text) for __aeabi_memclr4
    norflash.o(i.norflash_set_best_read_cfg) refers to norflash.o(i.norflash_en_quad) for norflash_en_quad
    norflash.o(i.norflash_set_best_read_cfg) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_set_best_read_cfg) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_set_best_write_cfg) refers to norflash.o(i.norflash_en_quad) for norflash_en_quad
    norflash.o(i.norflash_set_best_write_cfg) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_set_best_write_cfg) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_ddat_enable) for fls_ddat_enable
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_qdat_enable) for fls_qdat_enable
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_qadr_enable) for fls_qadr_enable
    norflash.o(i.norflash_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_write) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_write_disable) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_write_disable) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write_disable) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_write_disable) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_write_enable) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_write_enable) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write_enable) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_write_enable) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_big_end_enable) for norflash_big_end_enable
    norflash.o(i.norflash_write_endian_scr) refers to drv_fls.o(i.fls_en_scr) for fls_en_scr
    norflash.o(i.norflash_write_endian_scr) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_big_end_clear) for norflash_big_end_clear
    norflash.o(i.norflash_write_endian_scr) refers to drv_fls.o(i.fls_scr_clear) for fls_scr_clear
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_fifo_init) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_size) refers to dcs_packet_fifo.o(.bss) for .bss
    drv_common.o(i.app_HardFault_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_common.o(i.app_SysTick_Handler) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_enable_systick) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_common.o(i.drv_common_enable_systick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_get_tick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_system_init) refers to drv_chip_info.o(i.drv_chip_info_init) for drv_chip_info_init
    drv_common.o(i.drv_common_systick_register_cb) refers to drv_common.o(.data) for .data
    drv_dma.o(i.app_dma_irq_handler) refers to drv_dma.o(i.drv_dma_irq_handler) for drv_dma_irq_handler
    drv_dma.o(i.drv_dma_abort_transfer) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_abort_transfer) refers to drv_dma.o(i.drv_dma_disenable_channel_interrupts) for drv_dma_disenable_channel_interrupts
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_disenable_channel_interrupts) for drv_dma_disenable_channel_interrupts
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_clear_flag) for drv_dma_clear_flag
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_set_ccr) for drv_dma_set_ccr
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_dma.o(i.drv_dma_clear_flag) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.drv_dma_create_handle) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dma.o(i.drv_dma_disenable_channel_interrupts) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.drv_dma_enable_channel_interrupts) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dma.o(i.drv_dma_enable_cycle) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_get_remaining_bytes) refers to drv_dma.o(i.drv_dma_channel_is_active) for drv_dma_channel_is_active
    drv_dma.o(i.drv_dma_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dma.o(i.drv_dma_init) refers to drv_dma.o(i.drv_dma_ahb_init) for drv_dma_ahb_init
    drv_dma.o(i.drv_dma_irq_handler) refers to drv_dma.o(i.drv_dma_get_channel_flag) for drv_dma_get_channel_flag
    drv_dma.o(i.drv_dma_irq_handler) refers to drv_dma.o(i.drv_dma_clear_flag) for drv_dma_clear_flag
    drv_dma.o(i.drv_dma_irq_handler) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_m2m_init) refers to memseta.o(.text) for __aeabi_memclr4
    drv_dma.o(i.drv_dma_m2m_init) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    drv_dma.o(i.drv_dma_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_dma.o(i.drv_dma_set_burst) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_set_transfer) refers to drv_dma.o(i.drv_dma_set_burst) for drv_dma_set_burst
    drv_dma.o(i.drv_dma_start_transfer) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    drv_dma.o(i.drv_dma_start_transfer) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to ffltui.o(.text) for __aeabi_ui2f
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fdiv.o(.text) for __aeabi_fdiv
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fmul.o(.text) for __aeabi_fmul
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) for drv_dsi_rx_get_color_bpp
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc) for drv_dsi_rx_get_color_pcc
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fadd.o(.text) for __aeabi_fadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to cfrcmple.o(.text) for __aeabi_cfrcmple
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to f2d.o(.text) for __aeabi_f2d
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dadd.o(.text) for __aeabi_dadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dfixui.o(.text) for __aeabi_d2uiz
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte) for drv_rx_phy_test_write_1_byte
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to drv_dsi_rx.o(i.drv_rx_phy_test_read) for drv_rx_phy_test_read
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap) refers to drv_chip_info.o(i.drv_chip_info_get_info) for drv_chip_info_get_info
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_get_para) for drv_phy_get_para
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_clear) for drv_rx_phy_test_clear
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte) for drv_rx_phy_test_write_1_byte
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte) for drv_rx_phy_test_write_2_byte
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_chip_info.o(i.drv_chip_info_get_info) for drv_chip_info_get_info
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_lock) for drv_rx_phy_test_lock
    drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte) refers to drv_dsi_rx.o(i.drv_rx_phy_test_write) for drv_rx_phy_test_write
    drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte) refers to drv_dsi_rx.o(i.drv_rx_phy_test_write) for drv_rx_phy_test_write
    drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) for drv_tx_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to drv_dsi_tx.o(i.drv_tx_phy_test_read) for drv_tx_phy_test_read
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) for drv_tx_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_version) for drv_dsi_tx_version
    drv_dsi_tx.o(i.drv_dsi_tx_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dsi_tx.o(i.drv_tx_phy_test_write) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_code) for drv_tx_phy_test_write_code
    drv_dsi_tx.o(i.drv_tx_phy_test_write) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_data) for drv_tx_phy_test_write_data
    drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write) for drv_tx_phy_test_write
    drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write) for drv_tx_phy_test_write
    drv_fls.o(i.drv_fls_gpio_connect) refers to drv_fls.o(i.drv_fls_gpio_disconnect) for drv_fls_gpio_disconnect
    drv_fls.o(i.drv_fls_gpio_disconnect) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_EnableClk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_busy_pending) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    drv_fls.o(i.fls_de_init) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    drv_fls.o(i.fls_de_init) refers to drv_dma.o(i.drv_dma_clear_flag) for drv_dma_clear_flag
    drv_fls.o(i.fls_de_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_disable_it) refers to drv_fls.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_fls.o(i.fls_disable_it) refers to drv_fls.o(i.fls_set_mc_irq_mask) for fls_set_mc_irq_mask
    drv_fls.o(i.fls_enable_it) refers to drv_fls.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_fls.o(i.fls_enable_it) refers to drv_fls.o(i.fls_set_mc_irq_mask) for fls_set_mc_irq_mask
    drv_fls.o(i.fls_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_init) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_spi_init) for fls_spi_init
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_ctrl_cfg_init) for fls_ctrl_cfg_init
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_set_tuning) for fls_set_tuning
    drv_fls.o(i.fls_init) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_enable_it) for fls_enable_it
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_set_mc_irq_mask) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_fls.o(i.fls_set_mc_irq_mask) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_set_write) for fls_set_write
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_set_write) for fls_set_write
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect) for drv_ap_rst_trig_edge_detect
    drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_get_pull_state) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_register_ap_reset_callback) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.drv_gpio_register_callback) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_set_driving_strength) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_gpio.o(i.drv_gpio_set_pull_state) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_set_schmitt_trigger) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_set_slew_rate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_i2c_dma.o(i.drv_i2c_dma_callback) refers to drv_i2c_dma.o(.data) for .data
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_i2c_master.o(i.drv_i2c_m_enable) for drv_i2c_m_enable
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req) for drv_sys_cfg_set_dma_rx_req
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_dma.o(i.drv_dma_set_transfer) for drv_dma_set_transfer
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_i2c_dma.o(i.drv_i2c_master_write_read_cmd) for drv_i2c_master_write_read_cmd
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_dma.o(i.drv_dma_set_transfer) for drv_dma_set_transfer
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_i2c_dma.o(.data) for .data
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_i2c_dma.o(.bss) for .bss
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_i2c_dma.o(i.drv_i2c_dma_callback) for drv_i2c_dma_callback
    drv_i2c_dma.o(i.drv_i2c_slave_write_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_lcdc.o(i.drv_lcdc_config_scale_up_coef) refers to drv_param_init.o(i.drv_param_init_get_sclu_filter) for drv_param_init_get_sclu_filter
    drv_lcdc.o(i.drv_lcdc_config_src_parameter) refers to drv_lcdc.o(i.drv_lcdc_config_input_size) for drv_lcdc_config_input_size
    drv_lcdc.o(i.drv_lcdc_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_memc.o(i.app_MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_get_status) for drv_memc_get_status
    drv_memc.o(i.app_MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_clear_status) for drv_memc_clear_status
    drv_memc.o(i.app_MEMC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_param_init.o(i.drv_param_init_get_ccm) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_get_scld_filter_h) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_get_scld_filter_v) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_get_sclu_filter) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_set_ccm) refers to memcpya.o(.text) for __aeabi_memcpy4
    drv_param_init.o(i.drv_param_init_set_ccm) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_set_scld_filter) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_p2r_filter_init) refers to drv_param_init.o(.constdata) for .constdata
    drv_pwm.o(i.app_PWMDET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_pwm.o(i.app_PWMDET_IRQn_Handler) refers to drv_pwm.o(.data) for .data
    drv_pwm.o(i.drv_pwm_in_register_callback) refers to drv_pwm.o(.data) for .data
    drv_pwm.o(i.drv_pwm_in_set_sys_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_rxbr.o(i.app_ADC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.app_ADC_IRQn_Handler) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.app_VPRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.app_VPRE_IRQn_Handler) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_EnableIRQ) for __NVIC_EnableIRQ
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_rxbr.o(i.drv_rxbr_register_irq0_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_register_irq1_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_set_cmd_filter) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_rxbr.o(i.drv_rxbr_soft_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_dma.o(i.drv_dma_disenable_channel_interrupts) for drv_dma_disenable_channel_interrupts
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_master.o(i.drv_spi_m_enable_rx_dma) for drv_spi_m_enable_rx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_slave.o(i.drv_spi_s_enable_tx_dma) for drv_spi_s_enable_tx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_slave.o(i.drv_spi_s_enable_rx_dma) for drv_spi_s_enable_rx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_dma.o(i.drv_spi_dma_callback) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_dma_ch6_init) refers to drv_spi_dma.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_dma.o(i.drv_spi_dma_ch6_init) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_dma_init) refers to drv_spi_dma.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_dma.o(i.drv_spi_dma_init) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_spi_dma.o(i.drv_spi_dma_callback) for drv_spi_dma_callback
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_spi_dma.o(i.drv_spi_dma_callback) for drv_spi_dma_callback
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_spi_master.o(i.drv_spi_m_enable_rx_dma) for drv_spi_m_enable_rx_dma
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_spi_slave.o(i.drv_spi_s_enable_tx_dma) for drv_spi_s_enable_tx_dma
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_spi_dma.o(.bss) for .bss
    drv_swire.o(i.app_SWIRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_swire.o(i.app_SWIRE_IRQn_Handler) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    drv_swire.o(i.app_SWIRE_IRQn_Handler) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_register_callback) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig) for drv_sys_cfg_sel_ap_rst_lvl_trig
    drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect) refers to drv_sys_cfg.o(.data) for .data
    drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig) for drv_sys_cfg_sel_ap_rst_lvl_trig
    drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) refers to drv_sys_cfg.o(.data) for .data
    drv_timer.o(i.app_TIMER0_IRQn_Handler) refers to drv_timer.o(i.drv_timer_clear_status_flags) for drv_timer_clear_status_flags
    drv_timer.o(i.app_TIMER0_IRQn_Handler) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    drv_timer.o(i.app_TIMER0_IRQn_Handler) refers to drv_timer.o(.bss) for .bss
    drv_timer.o(i.app_TIMER1_IRQn_Handler) refers to drv_timer.o(i.drv_timer_clear_status_flags) for drv_timer_clear_status_flags
    drv_timer.o(i.app_TIMER1_IRQn_Handler) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    drv_timer.o(i.app_TIMER1_IRQn_Handler) refers to drv_timer.o(.bss) for .bss
    drv_timer.o(i.app_TIMER2_IRQn_Handler) refers to drv_timer.o(i.drv_timer_clear_status_flags) for drv_timer_clear_status_flags
    drv_timer.o(i.app_TIMER2_IRQn_Handler) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    drv_timer.o(i.app_TIMER2_IRQn_Handler) refers to drv_timer.o(.bss) for .bss
    drv_timer.o(i.app_TIMER3_IRQn_Handler) refers to drv_timer.o(i.drv_timer_clear_status_flags) for drv_timer_clear_status_flags
    drv_timer.o(i.app_TIMER3_IRQn_Handler) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    drv_timer.o(i.app_TIMER3_IRQn_Handler) refers to drv_timer.o(i.drv_timer_set_match) for drv_timer_set_match
    drv_timer.o(i.app_TIMER3_IRQn_Handler) refers to drv_timer.o(i.drv_timer_set_current_count) for drv_timer_set_current_count
    drv_timer.o(i.app_TIMER3_IRQn_Handler) refers to drv_timer.o(.bss) for .bss
    drv_timer.o(i.drv_timer_clean_timer_value) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_timer.o(i.drv_timer_enable) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_get_current_count) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_get_instance) refers to drv_timer.o(.constdata) for .constdata
    drv_timer.o(i.drv_timer_get_match) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_get_prescaler) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_register_callback) refers to drv_timer.o(.bss) for .bss
    drv_timer.o(i.drv_timer_set_current_count) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_timer.o(i.drv_timer_set_match) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_vidc.o(i.app_VIDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.app_VIDC_IRQn_Handler) refers to drv_vidc.o(.data) for .data
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_vidc.o(i.drv_vidc_register_callback) refers to drv_vidc.o(.data) for .data
    irq_redirect .o(i.ADC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.AP_NRESET_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.DMA_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT0_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT1_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT2_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT3_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT4_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT5_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT6_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT7_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.FLSCTRL_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.HardFault_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.I2C0_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.I2C1_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.LCDC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.MEMC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.MIPI_RX_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.MIPI_TX_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.PWMDET_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SPIM_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SPIS_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SWIRE_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SysTick_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER0_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER1_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER2_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER3_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.UART_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.VIDC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.VPRE_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.WDG_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.handle_init) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.handle_init) refers to drv_common.o(i.app_SysTick_Handler) for app_SysTick_Handler
    irq_redirect .o(i.handle_init) refers to hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) for app_LCDC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler) for app_MIPI_RX_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler) for app_MIPI_TX_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_dma.o(i.app_dma_irq_handler) for app_dma_irq_handler
    irq_redirect .o(i.handle_init) refers to norflash.o(i.app_fls_ctrl_Handler) for app_fls_ctrl_Handler
    irq_redirect .o(i.handle_init) refers to drv_i2c_slave.o(i.app_I2C0_IRQn_Handler) for app_I2C0_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_i2c_master.o(i.app_I2C1_IRQn_Handler) for app_I2C1_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to hal_spi_slave.o(i.app_SPIS_IRQn_Handler) for app_SPIS_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_spi_master.o(i.app_SPIM_IRQn_Handler) for app_SPIM_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_rxbr.o(i.app_VPRE_IRQn_Handler) for app_VPRE_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_rxbr.o(i.app_ADC_IRQn_Handler) for app_ADC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_vidc.o(i.app_VIDC_IRQn_Handler) for app_VIDC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_memc.o(i.app_MEMC_IRQn_Handler) for app_MEMC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER0_IRQn_Handler) for app_TIMER0_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER1_IRQn_Handler) for app_TIMER1_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER2_IRQn_Handler) for app_TIMER2_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER3_IRQn_Handler) for app_TIMER3_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_wdg.o(i.app_WDG_IRQn_Handler) for app_WDG_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_uart.o(i.app_UART_IRQn_Handler) for app_UART_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_pwm.o(i.app_PWMDET_IRQn_Handler) for app_PWMDET_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_swire.o(i.app_SWIRE_IRQn_Handler) for app_SWIRE_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) for app_AP_NRESET_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler) for app_EXTI_INT0_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler) for app_EXTI_INT1_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler) for app_EXTI_INT2_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler) for app_EXTI_INT3_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler) for app_EXTI_INT4_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler) for app_EXTI_INT5_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler) for app_EXTI_INT6_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler) for app_EXTI_INT7_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_common.o(i.app_HardFault_Handler) for app_HardFault_Handler
    drv_phy_common.o(i.drv_phy_get_calibration) refers to drv_chip_info.o(i.drv_chip_info_get_info) for drv_chip_info_get_info
    drv_phy_common.o(i.drv_phy_get_calibration) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_phy_common.o(i.drv_phy_get_calibration) refers to drv_phy_common.o(.data) for .data
    drv_phy_common.o(i.drv_phy_get_para) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_phy_common.o(i.drv_phy_get_para) refers to drv_phy_common.o(.constdata) for .constdata
    drv_i2c_master.o(i.app_I2C1_IRQn_Handler) refers to drv_i2c_master.o(.data) for .data
    drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_enable_intr) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_read_data) refers to drv_i2c_master.o(i.drv_i2c_m_get_fifo_status) for drv_i2c_m_get_fifo_status
    drv_i2c_master.o(i.drv_i2c_m_set_callback) refers to drv_i2c_master.o(.data) for .data
    drv_i2c_master.o(i.drv_i2c_m_set_sys_mask) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_write_data) refers to drv_i2c_master.o(i.drv_i2c_m_get_fifo_status) for drv_i2c_m_get_fifo_status
    drv_i2c_master.o(i.drv_i2c_master_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_i2c_master.o(i.drv_i2c_master_init) refers to drv_common.o(.data) for g_system_clock
    drv_i2c_slave.o(i.app_I2C0_IRQn_Handler) refers to drv_i2c_slave.o(.data) for .data
    drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit) refers to drv_i2c_slave.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_slave.o(i.drv_i2c_s_enable_intr) refers to drv_i2c_slave.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_slave.o(i.drv_i2c_s_get_tx_byte_num) refers to drv_i2c_slave.o(.data) for .data
    drv_i2c_slave.o(i.drv_i2c_s_read_data) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    drv_i2c_slave.o(i.drv_i2c_s_set_callback) refers to drv_i2c_slave.o(.data) for .data
    drv_i2c_slave.o(i.drv_i2c_s_set_sys_mask) refers to drv_i2c_slave.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_slave.o(i.drv_i2c_s_write_data) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    drv_spi_master.o(i.app_SPIM_IRQn_Handler) refers to drv_spi_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_master.o(i.app_SPIM_IRQn_Handler) refers to drv_spi_master.o(.data) for .data
    drv_spi_master.o(i.drv_spi_m_deinit) refers to drv_spi_master.o(i.drv_spi_m_switch_sclk) for drv_spi_m_switch_sclk
    drv_spi_master.o(i.drv_spi_m_disable_int) refers to drv_spi_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_master.o(i.drv_spi_m_set_intr_callback) refers to drv_spi_master.o(.data) for .data
    drv_spi_master.o(i.drv_spi_master_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_spi_master.o(i.drv_spi_master_init) refers to drv_common.o(.data) for g_system_clock
    drv_chip_info.o(i.drv_chip_info_get_info) refers to drv_chip_info.o(.data) for .data
    drv_chip_info.o(i.drv_chip_info_init) refers to drv_efuse.o(i.drv_efuse_enter_inactive) for drv_efuse_enter_inactive
    drv_chip_info.o(i.drv_chip_info_init) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_chip_info.o(i.drv_chip_info_init) refers to drv_chip_info.o(.data) for .data
    drv_chip_info.o(i.drv_chip_rx_info_check) refers to printfa.o(i.__0printf) for __2printf
    drv_chip_info.o(i.drv_chip_rx_info_check) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_chip_info.o(i.drv_chip_rx_info_check) refers to drv_chip_info.o(.data) for .data
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to drv_efuse.o(i.drv_efuse_enter_inactive) for drv_efuse_enter_inactive
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to printfa.o(i.__0printf) for __2printf
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to hal_spi_slave.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_spi_slave.o(i.hal_spi_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    hal_spi_slave.o(i.hal_spi_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_abort) refers to drv_spi_dma.o(i.drv_spi_abort_dma) for drv_spi_abort_dma
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start) refers to drv_dma.o(i.drv_dma_enable_cycle) for drv_dma_enable_cycle
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start) refers to drv_spi_dma.o(i.drv_spis_dma_write) for drv_spis_dma_write
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_deinit) refers to drv_spi_slave.o(i.drv_spi_s_deinit) for drv_spi_s_deinit
    hal_spi_slave.o(i.hal_spi_slave_enable) refers to drv_spi_slave.o(i.drv_spi_s_enable_int) for drv_spi_s_enable_int
    hal_spi_slave.o(i.hal_spi_slave_enable) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_spi_slave.o(i.hal_spi_slave_enable) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_gpio_init) refers to drv_spi_slave.o(i.drv_spi_s_gpio_init) for drv_spi_s_gpio_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to hal_spi_slave.o(i.hal_spi_slave_gpio_init) for hal_spi_slave_gpio_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_slave.o(i.drv_spi_slave_init) for drv_spi_slave_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_dma.o(i.drv_spi_dma_init) for drv_spi_dma_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) for drv_spi_set_dma_irq_callback
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_slave.o(i.drv_spi_s_enable_tx_dma) for drv_spi_s_enable_tx_dma
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    hal_spi_slave.o(i.hal_spi_slave_init) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_read_data) refers to drv_spi_slave.o(i.drv_spi_s_read_data) for drv_spi_s_read_data
    hal_spi_slave.o(i.hal_spi_slave_register_callback) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_reset_tx) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_set_auto_rx_buffer) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_set_auto_tx_buffer) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_write_data) refers to drv_spi_slave.o(i.drv_spi_s_write_data) for drv_spi_s_write_data
    drv_fls_dma.o(i.fls_abort_dma) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_fls_dma.o(i.fls_abort_dma) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls_dma.o(i.fls_dma_enable) for fls_dma_enable
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_set_write) for fls_set_write
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls_dma.o(i.fls_dma_enable) for fls_dma_enable
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls_dma.o(i.fls_read_dmacallback) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to memseta.o(.text) for __aeabi_memclr4
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_fls_dma.o(.data) for .data
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_fls_dma.o(i.fls_read_dmacallback) for fls_read_dmacallback
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_fls_dma.o(i.fls_write_dmacallback) for fls_write_dmacallback
    drv_fls_dma.o(i.fls_transfer_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_fls_dma.o(i.fls_transfer_dma) refers to drv_dma.o(i.drv_dma_start_transfer) for drv_dma_start_transfer
    drv_fls_dma.o(i.fls_transfer_get_receive_count_dma) refers to drv_dma.o(i.drv_dma_get_remaining_bytes) for drv_dma_get_remaining_bytes
    drv_fls_dma.o(i.fls_write_dmacallback) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_uart.o(i.UART0_IRQ_Handle) refers to drv_uart.o(i.UART_TransferHandleIRQ) for UART_TransferHandleIRQ
    drv_uart.o(i.UART0_IRQ_Handle) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_uart.o(i.UART0_IRQ_Handle) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_AbortReceive) refers to drv_uart.o(i.UART_Disable_IT) for UART_Disable_IT
    drv_uart.o(i.UART_AbortReceive) refers to drv_uart.o(i.UART_ResetRxFIFO) for UART_ResetRxFIFO
    drv_uart.o(i.UART_AbortSend) refers to drv_uart.o(i.UART_Disable_IT) for UART_Disable_IT
    drv_uart.o(i.UART_AbortSend) refers to drv_uart.o(i.UART_ResetTxFIFO) for UART_ResetTxFIFO
    drv_uart.o(i.UART_Deinit) refers to drv_uart.o(i.UART_SwitchSCLK) for UART_SwitchSCLK
    drv_uart.o(i.UART_Disable_IT) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_Disable_IT) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.UART_Disable_IT) refers to drv_uart.o(.constdata) for .constdata
    drv_uart.o(i.UART_EnableDma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req) for drv_sys_cfg_set_dma_rx_req
    drv_uart.o(i.UART_EnableDma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    drv_uart.o(i.UART_Enable_IT) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_Enable_IT) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.UART_GetDefaultConfig) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.UART_GetDefaultConfig) refers to drv_common.o(.data) for g_system_clock
    drv_uart.o(i.UART_GetFIFO_Ctrl) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_GetFIFO_Ctrl) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_ResetRxFIFO) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_ResetRxFIFO) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_ResetTxFIFO) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_ResetTxFIFO) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_SetBaudRate) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_uart.o(i.UART_SwitchSCLK) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_uart.o(i.UART_TransferCreateHandle) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_TransferCreateHandle) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.UART_TransferCreateHandle) refers to drv_uart.o(i.UART_Enable_IT) for UART_Enable_IT
    drv_uart.o(i.UART_TransferCreateHandle) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_TransferHandleIRQ) refers to drv_uart.o(i.UART_ResetRxFIFO) for UART_ResetRxFIFO
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_DisableDma) for UART_DisableDma
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_SwitchSCLK) for UART_SwitchSCLK
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_SetBaudRate) for UART_SetBaudRate
    drv_uart.o(i.UART_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.UART_init) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.app_UART_IRQn_Handler) refers to drv_uart.o(i.UART0_IRQ_Handle) for UART0_IRQ_Handle
    drv_uart_dma.o(i.UART_DMAInit) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart_dma.o(i.UART_DMAInit) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    drv_uart_dma.o(i.UART_TransferAbortReceiveDMA) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_uart_dma.o(i.UART_TransferAbortSendDMA) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart.o(i.UART_EnableDma) for UART_EnableDma
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(i.UART_DMAInit) for UART_DMAInit
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(.data) for .data
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(i.UART_TransferReceiveDMACallback) for UART_TransferReceiveDMACallback
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(i.UART_TransferSendDMACallback) for UART_TransferSendDMACallback
    drv_uart_dma.o(i.UART_TransferGetReceiveCountDMA) refers to drv_dma.o(i.drv_dma_get_remaining_bytes) for drv_dma_get_remaining_bytes
    drv_uart_dma.o(i.UART_TransferReceiveDMA) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_uart_dma.o(i.UART_TransferReceiveDMA) refers to drv_uart.o(i.UART_EnableDma) for UART_EnableDma
    drv_uart_dma.o(i.UART_TransferReceiveDMA) refers to drv_dma.o(i.drv_dma_start_transfer) for drv_dma_start_transfer
    drv_uart_dma.o(i.UART_TransferSendDMA) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_uart_dma.o(i.UART_TransferSendDMA) refers to drv_uart.o(i.UART_EnableDma) for UART_EnableDma
    drv_uart_dma.o(i.UART_TransferSendDMA) refers to drv_dma.o(i.drv_dma_start_transfer) for drv_dma_start_transfer
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_read_edge_flag) for drv_wdg_read_edge_flag
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_clear_edge_flag) for drv_wdg_clear_edge_flag
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_set_int) for drv_wdg_set_int
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(.data) for .data
    drv_wdg.o(i.drv_wdg_register_callback) refers to drv_wdg.o(.data) for .data
    drv_wdg.o(i.drv_wdg_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_efuse.o(i.drv_efuse_enter_inactive) refers to drv_efuse.o(i.drv_efuse_int_enable) for drv_efuse_int_enable
    drv_efuse.o(i.drv_efuse_read) refers to drv_efuse.o(i.drv_efuse_read_req) for drv_efuse_read_req
    drv_efuse.o(i.drv_efuse_write) refers to drv_efuse.o(i.drv_efuse_write_req) for drv_efuse_write_req
    drv_spi_slave.o(i.drv_spi_s_deinit) refers to drv_spi_slave.o(i.drv_spi_s_switch_sclk) for drv_spi_s_switch_sclk
    ceil.o(i.__softfp_ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.__softfp_ceil) refers to ceil.o(i.ceil) for ceil
    ceil.o(i.ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.ceil) refers to dadd.o(.text) for __aeabi_dadd
    ceil.o(i.ceil) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry10a.o(.ARM.Collect$$$$0000000D) for __rt_final_cpp
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry11a.o(.ARM.Collect$$$$0000000F) for __rt_final_exit
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry7b.o(.ARM.Collect$$$$00000008) for _main_clock
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry8b.o(.ARM.Collect$$$$0000000A) for _main_cpp_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry9a.o(.ARM.Collect$$$$0000000B) for _main_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry5.o(.ARM.Collect$$$$00000004) for _main_scatterload
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry2.o(.ARM.Collect$$$$00000001) for _main_stk
    idiv.o(.text) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfb.o(i.__0fprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0fprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0printf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printfb.o(i.__0vfprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vfprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printf0.o(i.__0fprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0fprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0printf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf0.o(i.__0vfprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vfprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf1.o(i.__0fprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0fprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0printf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i.__0vfprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vfprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf2.o(i.__0fprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0fprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0printf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf2.o(i.__0vfprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vfprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf3.o(i.__0fprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0fprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0printf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i.__0vfprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vfprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf4.o(i.__0fprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0fprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0printf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i.__0vfprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vfprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf5.o(i.__0fprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0fprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0printf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i.__0vfprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vfprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf6.o(i.__0fprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0fprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0printf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i.__0vfprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vfprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i._printf_core) refers to printf6.o(i._printf_pre_padding) for _printf_pre_padding
    printf6.o(i._printf_core) refers to printf6.o(i._printf_post_padding) for _printf_post_padding
    printf6.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf7.o(i.__0fprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0fprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0printf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i.__0vfprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vfprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i._printf_core) refers to printf7.o(i._printf_pre_padding) for _printf_pre_padding
    printf7.o(i._printf_core) refers to printf7.o(i._printf_post_padding) for _printf_post_padding
    printf7.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf8.o(i.__0fprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0fprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0printf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i.__0vfprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vfprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i._printf_core) refers to printf8.o(i._printf_pre_padding) for _printf_pre_padding
    printf8.o(i._printf_core) refers to printf8.o(i._printf_post_padding) for _printf_post_padding
    printf8.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i.__0fprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0fprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0fprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0printf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0printf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0snprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0snprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0snprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0sprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0sprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0sprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i.__0vfprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vfprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vfprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0vsnprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0vsprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i._fp_digits) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._fp_digits) refers to dmul.o(.text) for __aeabi_dmul
    printfa.o(i._fp_digits) refers to ddiv.o(.text) for __aeabi_ddiv
    printfa.o(i._fp_digits) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    printfa.o(i._fp_digits) refers to dadd.o(.text) for __aeabi_dadd
    printfa.o(i._fp_digits) refers to dfixul.o(.text) for __aeabi_d2ulz
    printfa.o(i._fp_digits) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_core) refers to printfa.o(i._printf_pre_padding) for _printf_pre_padding
    printfa.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers to printfa.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i._printf_core) refers to printfa.o(i._fp_digits) for _fp_digits
    printfa.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfa.o(i._printf_post_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_pre_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._snputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._sputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    fmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers to fepilogue.o(.text) for _float_round
    fscalb.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    dadd.o(.text) refers to llsshr.o(.text) for __aeabi_lasr
    dadd.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dmul.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ddiv.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ddiv.o(.text) refers to depilogue.o(.text) for _double_round
    fflti.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fflti.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    ffltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ffltui.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    dflti.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dflti.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dfltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfltui.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ffixi.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ffixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixi.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixi.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixui.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    f2d.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    cfrcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    entry2.o(.ARM.Collect$$$$00000001) refers to entry2.o(.ARM.Collect$$$$00002712) for __lit__00000000
    entry2.o(.ARM.Collect$$$$00002712) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    entry5.o(.ARM.Collect$$$$00000004) refers to init.o(.text) for __scatterload
    entry9a.o(.ARM.Collect$$$$0000000B) refers to main.o(i.main) for main
    entry9b.o(.ARM.Collect$$$$0000000C) refers to main.o(i.main) for main
    uldiv.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    uldiv.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to depilogue.o(i.__ARM_clz) for __ARM_clz
    depilogue.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixul.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixul.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    init.o(.text) refers to entry5.o(.ARM.Collect$$$$00000004) for __main_after_scatterload


==============================================================================

Removing Unused input sections from the image.

    Removing main.o(.rev16_text), (4 bytes).
    Removing main.o(.revsh_text), (4 bytes).
    Removing ap_demo.o(.rev16_text), (4 bytes).
    Removing ap_demo.o(.revsh_text), (4 bytes).
    Removing ap_demo.o(i.PWM_OUTPUT_TEST), (44 bytes).
    Removing ap_demo.o(i.test_pwm_out_adjust), (104 bytes).
    Removing ap_demo.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.rev16_text), (4 bytes).
    Removing app_tp_for_custom_s8.o(.revsh_text), (4 bytes).
    Removing app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const), (156 bytes).
    Removing app_tp_for_custom_s8.o(.bss), (200 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (4 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (8 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (37 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (1 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (3 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (3 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (11 bytes).
    Removing app_tp_for_custom_s8.o(.data), (10 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (64 bytes).
    Removing app_tp_for_custom_s8.o(.data), (3 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (32 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (16 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_transfer.o(.rev16_text), (4 bytes).
    Removing app_tp_transfer.o(.revsh_text), (4 bytes).
    Removing app_tp_transfer.o(i.app_tp_m_transfer_complate), (8 bytes).
    Removing app_tp_transfer.o(i.app_tp_phone_reset_on), (12 bytes).
    Removing app_tp_transfer.o(i.app_tp_s_transfer_complate), (26 bytes).
    Removing app_tp_transfer.o(.bss), (200 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (5 bytes).
    Removing app_tp_transfer.o(.data), (6 bytes).
    Removing app_tp_transfer.o(.data), (2 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (1 bytes).
    Removing app_tp_transfer.o(.data), (2 bytes).
    Removing app_tp_transfer.o(.data), (2 bytes).
    Removing board.o(.rev16_text), (4 bytes).
    Removing board.o(.revsh_text), (4 bytes).
    Removing startup_armcm0.o(HEAP), (3072 bytes).
    Removing hal_dsi_rx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd), (88 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_short_cmd), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video), (228 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init), (48 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern), (216 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en), (16 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode), (172 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle), (40 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart), (80 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter), (108 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_dcs_direct_mode), (8 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter), (40 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format), (56 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data), (148 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_te_waveform), (52 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex), (14 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate), (112 bytes).
    Removing hal_dsi_tx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_ulps_mode), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_ulps_mode), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd), (156 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle), (28 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_lp_cmd), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg), (24 bytes).
    Removing hal_gpio.o(.rev16_text), (4 bytes).
    Removing hal_gpio.o(.revsh_text), (4 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_int_type), (20 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_pull_state), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_init_input), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_driving_strength), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_output_data_ex), (36 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_schmitt_trigger), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_slew_rate), (32 bytes).
    Removing hal_pwm.o(.rev16_text), (4 bytes).
    Removing hal_pwm.o(.revsh_text), (4 bytes).
    Removing hal_pwm.o(i.hal_pwm_in_clear_int), (8 bytes).
    Removing hal_pwm.o(i.hal_pwm_in_config_int), (60 bytes).
    Removing hal_pwm.o(i.hal_pwm_in_ctrl_int), (8 bytes).
    Removing hal_pwm.o(i.hal_pwm_in_deinit), (18 bytes).
    Removing hal_pwm.o(i.hal_pwm_in_get_current_count), (8 bytes).
    Removing hal_pwm.o(i.hal_pwm_in_get_high_period), (40 bytes).
    Removing hal_pwm.o(i.hal_pwm_in_get_low_period), (40 bytes).
    Removing hal_pwm.o(i.hal_pwm_in_get_total_period), (40 bytes).
    Removing hal_pwm.o(i.hal_pwm_in_init), (26 bytes).
    Removing hal_pwm.o(i.hal_pwm_in_register_callback), (10 bytes).
    Removing hal_pwm.o(i.hal_pwm_in_set_int), (8 bytes).
    Removing hal_pwm.o(i.hal_pwm_out_deinit), (18 bytes).
    Removing hal_pwm.o(i.hal_pwm_out_pause), (8 bytes).
    Removing hal_pwm.o(i.hal_pwm_out_sel_io), (38 bytes).
    Removing hal_pwm.o(i.hal_pwm_out_sync_all), (124 bytes).
    Removing hal_pwm.o(i.hal_pwm_out_sync_ctl), (32 bytes).
    Removing hal_pwm.o(i.hal_pwm_out_sync_pause), (28 bytes).
    Removing hal_pwm.o(i.hal_pwm_out_sync_period), (52 bytes).
    Removing hal_pwm.o(i.hal_pwm_out_sync_thr), (72 bytes).
    Removing hal_swire.o(.rev16_text), (4 bytes).
    Removing hal_swire.o(.revsh_text), (4 bytes).
    Removing hal_swire.o(i.hal_swire_deinit), (18 bytes).
    Removing hal_swire.o(i.hal_swire_init), (32 bytes).
    Removing hal_swire.o(i.hal_swire_register_callback), (10 bytes).
    Removing hal_swire.o(i.hal_swire_start), (112 bytes).
    Removing hal_system.o(.rev16_text), (4 bytes).
    Removing hal_system.o(.revsh_text), (4 bytes).
    Removing hal_system.o(i.cvt_cfg_packet), (24 bytes).
    Removing hal_system.o(i.cvt_check_cgf_is_valid), (42 bytes).
    Removing hal_system.o(i.hal_system_deep_sleep_mode), (8 bytes).
    Removing hal_system.o(i.hal_system_disable_systick), (8 bytes).
    Removing hal_system.o(i.hal_system_flash_read), (60 bytes).
    Removing hal_system.o(i.hal_system_flash_write), (64 bytes).
    Removing hal_system.o(i.hal_system_get_tick), (8 bytes).
    Removing hal_system.o(i.hal_system_idle_mode), (8 bytes).
    Removing hal_system.o(i.hal_system_register_systick_cb), (8 bytes).
    Removing hal_system.o(i.hal_system_reset_chip), (32 bytes).
    Removing hal_system.o(i.hal_system_share_flash_mode), (20 bytes).
    Removing hal_system.o(i.hal_system_sleep_mode), (48 bytes).
    Removing hal_timer.o(.rev16_text), (4 bytes).
    Removing hal_timer.o(.revsh_text), (4 bytes).
    Removing hal_timer.o(i.hal_timer_deinit), (24 bytes).
    Removing hal_timer.o(i.hal_timer_get_status), (52 bytes).
    Removing hal_i2c_master.o(.rev16_text), (4 bytes).
    Removing hal_i2c_master.o(.revsh_text), (4 bytes).
    Removing hal_i2c_master.o(i.hal_i2c_m_set_high_impedance), (46 bytes).
    Removing hal_i2c_slave.o(.rev16_text), (4 bytes).
    Removing hal_i2c_slave.o(.revsh_text), (4 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_get_tx_byte_num), (8 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_read_complate), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_read_complate_clear), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_read_data), (8 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_rxfifo_notempty), (20 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_set_dma_tx_cycle), (36 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance), (46 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_write_complate), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_write_data), (8 bytes).
    Removing hal_spi_master.o(.rev16_text), (4 bytes).
    Removing hal_spi_master.o(.revsh_text), (4 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_callback), (24 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_dma_init), (104 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_dma_read), (36 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_dma_write), (40 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_get_transfer_complate), (36 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_gpio_init), (8 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_read_rxfifo), (28 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_set_high_impedance), (100 bytes).
    Removing hal_spi_master.o(.data), (1 bytes).
    Removing tau_delay.o(.rev16_text), (4 bytes).
    Removing tau_delay.o(.revsh_text), (4 bytes).
    Removing tau_log.o(.rev16_text), (4 bytes).
    Removing tau_log.o(.revsh_text), (4 bytes).
    Removing tau_log.o(i.fgetc), (22 bytes).
    Removing hal_uart.o(.rev16_text), (4 bytes).
    Removing hal_uart.o(.revsh_text), (4 bytes).
    Removing hal_uart.o(i.hal_uart_deinit), (28 bytes).
    Removing hal_uart.o(i.hal_uart_dmacallback), (36 bytes).
    Removing hal_uart.o(i.hal_uart_receive_blocking), (16 bytes).
    Removing hal_uart.o(i.hal_uart_receive_dma), (76 bytes).
    Removing hal_uart.o(i.hal_uart_transmit_dma), (76 bytes).
    Removing hal_internal_vsync.o(.rev16_text), (4 bytes).
    Removing hal_internal_vsync.o(.revsh_text), (4 bytes).
    Removing hal_internal_vsync.o(i.hal_iniernal_vsync_deinit), (20 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual), (528 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state), (12 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state), (12 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode), (48 bytes).
    Removing norflash.o(.rev16_text), (4 bytes).
    Removing norflash.o(.revsh_text), (4 bytes).
    Removing norflash.o(i.norflash_best_cfg_init), (44 bytes).
    Removing norflash.o(i.norflash_big_end_clear), (14 bytes).
    Removing norflash.o(i.norflash_big_end_enable), (20 bytes).
    Removing norflash.o(i.norflash_check_crc32), (14 bytes).
    Removing norflash.o(i.norflash_check_id), (72 bytes).
    Removing norflash.o(i.norflash_dma_callback), (24 bytes).
    Removing norflash.o(i.norflash_dma_read), (156 bytes).
    Removing norflash.o(i.norflash_dma_write), (252 bytes).
    Removing norflash.o(i.norflash_dual_read), (60 bytes).
    Removing norflash.o(i.norflash_dual_write), (112 bytes).
    Removing norflash.o(i.norflash_en4b), (40 bytes).
    Removing norflash.o(i.norflash_en_quad), (116 bytes).
    Removing norflash.o(i.norflash_en_quad_check), (64 bytes).
    Removing norflash.o(i.norflash_erase_block), (44 bytes).
    Removing norflash.o(i.norflash_erase_chip), (28 bytes).
    Removing norflash.o(i.norflash_erase_sector), (44 bytes).
    Removing norflash.o(i.norflash_ex4b), (40 bytes).
    Removing norflash.o(i.norflash_exit_quad), (76 bytes).
    Removing norflash.o(i.norflash_get_dual_hstatus), (52 bytes).
    Removing norflash.o(i.norflash_get_hstatus), (52 bytes).
    Removing norflash.o(i.norflash_get_status), (52 bytes).
    Removing norflash.o(i.norflash_init), (48 bytes).
    Removing norflash.o(i.norflash_quad_read), (76 bytes).
    Removing norflash.o(i.norflash_quad_write), (108 bytes).
    Removing norflash.o(i.norflash_read), (28 bytes).
    Removing norflash.o(i.norflash_read_config_reg), (36 bytes).
    Removing norflash.o(i.norflash_read_id), (20 bytes).
    Removing norflash.o(i.norflash_reset), (2 bytes).
    Removing norflash.o(i.norflash_reset_crc32), (32 bytes).
    Removing norflash.o(i.norflash_set_best_cfg), (50 bytes).
    Removing norflash.o(i.norflash_set_best_read_cfg), (84 bytes).
    Removing norflash.o(i.norflash_set_best_write_cfg), (84 bytes).
    Removing norflash.o(i.norflash_switch_fls_spi), (112 bytes).
    Removing norflash.o(i.norflash_write), (96 bytes).
    Removing norflash.o(i.norflash_write_disable), (64 bytes).
    Removing norflash.o(i.norflash_write_enable), (56 bytes).
    Removing norflash.o(i.norflash_write_endian_scr), (132 bytes).
    Removing norflash.o(.bss), (412 bytes).
    Removing norflash.o(.bss), (32 bytes).
    Removing norflash.o(.data), (2 bytes).
    Removing dcs_packet_fifo.o(i.dcs_packet_get_fifo_size), (16 bytes).
    Removing drv_common.o(.rev16_text), (4 bytes).
    Removing drv_common.o(.revsh_text), (4 bytes).
    Removing drv_common.o(i.drv_common_disable_systick), (20 bytes).
    Removing drv_common.o(i.drv_common_get_tick), (12 bytes).
    Removing drv_common.o(i.drv_common_idle_mode), (40 bytes).
    Removing drv_common.o(i.drv_common_systick_register_cb), (12 bytes).
    Removing drv_crgu.o(.rev16_text), (4 bytes).
    Removing drv_crgu.o(.revsh_text), (4 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_reset_flag), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_config_clocks), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_config_clocks_div), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_config_clocks_src), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_ana_clk_status), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_fpga_id), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_mipi_ref_src), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_reset_flag), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_system_clk), (28 bytes).
    Removing drv_crgu.o(i.drv_crgu_reset_chip), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_200m_scan_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_300m_scan_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_abp0_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_adc_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_adc_src), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_apb1_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_apb2_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_fls_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_fls_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_monitor_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_monitor_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_swire_div), (20 bytes).
    Removing drv_dma.o(.rev16_text), (4 bytes).
    Removing drv_dma.o(.revsh_text), (4 bytes).
    Removing drv_dma.o(i.drv_dma_abort_transfer), (32 bytes).
    Removing drv_dma.o(i.drv_dma_ahb_init), (74 bytes).
    Removing drv_dma.o(i.drv_dma_channel_is_active), (20 bytes).
    Removing drv_dma.o(i.drv_dma_deinit), (32 bytes).
    Removing drv_dma.o(i.drv_dma_disenable_channel_interrupts), (24 bytes).
    Removing drv_dma.o(i.drv_dma_enable_cycle), (44 bytes).
    Removing drv_dma.o(i.drv_dma_get_remaining_bytes), (32 bytes).
    Removing drv_dma.o(i.drv_dma_init), (24 bytes).
    Removing drv_dma.o(i.drv_dma_m2m_init), (72 bytes).
    Removing drv_dma.o(i.drv_dma_reset), (10 bytes).
    Removing drv_dma.o(i.drv_dma_set_ccr), (114 bytes).
    Removing drv_dma.o(i.drv_dma_start_transfer), (32 bytes).
    Removing drv_dsi_rx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_rx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate), (66 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_version), (4 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration), (236 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg), (32 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg), (48 bytes).
    Removing drv_dsi_rx.o(i.drv_rx_phy_test_read), (12 bytes).
    Removing drv_dsi_tx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_tx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_force_interrupt), (8 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_get_phy_status), (6 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_forcepll), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration), (232 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_start), (18 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock), (10 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot), (62 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger), (92 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter), (344 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit), (276 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_sdf_3d), (28 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_bta), (22 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_vpg), (70 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_version), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_vid_shadow), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_lock), (30 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_read), (10 bytes).
    Removing drv_fls.o(.rev16_text), (4 bytes).
    Removing drv_fls.o(.revsh_text), (4 bytes).
    Removing drv_fls.o(i.__NVIC_DisableIRQ), (32 bytes).
    Removing drv_fls.o(i.drv_fls_gpio_connect), (28 bytes).
    Removing drv_fls.o(i.drv_fls_gpio_disconnect), (32 bytes).
    Removing drv_fls.o(i.fls_EnableClk), (12 bytes).
    Removing drv_fls.o(i.fls_busy_pending), (12 bytes).
    Removing drv_fls.o(i.fls_clear_irq_status), (6 bytes).
    Removing drv_fls.o(i.fls_ctrl_cfg_init), (72 bytes).
    Removing drv_fls.o(i.fls_ddat_enable), (24 bytes).
    Removing drv_fls.o(i.fls_de_init), (52 bytes).
    Removing drv_fls.o(i.fls_descr), (10 bytes).
    Removing drv_fls.o(i.fls_disable_it), (36 bytes).
    Removing drv_fls.o(i.fls_en_scr), (10 bytes).
    Removing drv_fls.o(i.fls_enable_it), (48 bytes).
    Removing drv_fls.o(i.fls_get_crcout), (4 bytes).
    Removing drv_fls.o(i.fls_get_default_fls_config), (20 bytes).
    Removing drv_fls.o(i.fls_get_default_spi_config), (44 bytes).
    Removing drv_fls.o(i.fls_get_default_tuning), (12 bytes).
    Removing drv_fls.o(i.fls_get_tuning), (18 bytes).
    Removing drv_fls.o(i.fls_init), (62 bytes).
    Removing drv_fls.o(i.fls_qadr_enable), (22 bytes).
    Removing drv_fls.o(i.fls_qcmd_enable), (22 bytes).
    Removing drv_fls.o(i.fls_qdat_enable), (22 bytes).
    Removing drv_fls.o(i.fls_read_byte_data), (130 bytes).
    Removing drv_fls.o(i.fls_read_cmd), (104 bytes).
    Removing drv_fls.o(i.fls_read_cmd_it), (110 bytes).
    Removing drv_fls.o(i.fls_reset_crc), (18 bytes).
    Removing drv_fls.o(i.fls_scr_clear), (10 bytes).
    Removing drv_fls.o(i.fls_set_addr_dummy), (32 bytes).
    Removing drv_fls.o(i.fls_set_addr_len), (32 bytes).
    Removing drv_fls.o(i.fls_set_mc_irq_mask), (26 bytes).
    Removing drv_fls.o(i.fls_set_read), (10 bytes).
    Removing drv_fls.o(i.fls_set_tuning), (24 bytes).
    Removing drv_fls.o(i.fls_set_write), (10 bytes).
    Removing drv_fls.o(i.fls_single_mode), (16 bytes).
    Removing drv_fls.o(i.fls_spi_init), (180 bytes).
    Removing drv_fls.o(i.fls_spi_start), (10 bytes).
    Removing drv_fls.o(i.fls_swrst), (18 bytes).
    Removing drv_fls.o(i.fls_write_byte_data), (164 bytes).
    Removing drv_fls.o(i.fls_write_cmd), (58 bytes).
    Removing drv_fls.o(.data), (4 bytes).
    Removing drv_gpio.o(.rev16_text), (4 bytes).
    Removing drv_gpio.o(.revsh_text), (4 bytes).
    Removing drv_gpio.o(i.drv_gpio_get_pull_state), (224 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_driving_strength), (312 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_schmitt_trigger), (168 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_slew_rate), (168 bytes).
    Removing drv_i2c_dma.o(.rev16_text), (4 bytes).
    Removing drv_i2c_dma.o(.revsh_text), (4 bytes).
    Removing drv_lcdc.o(.rev16_text), (4 bytes).
    Removing drv_lcdc.o(.revsh_text), (4 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_config_rgb_to_pentile), (26 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_enable), (42 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_set_prefetch), (24 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_update_shadow_reg), (12 bytes).
    Removing drv_memc.o(.rev16_text), (4 bytes).
    Removing drv_memc.o(.revsh_text), (4 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_frm_time), (14 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_int_frame), (28 bytes).
    Removing drv_memc.o(i.drv_memc_set_fb_remaining_line_trigger), (12 bytes).
    Removing drv_memc.o(i.drv_memc_set_read_trigger_line), (16 bytes).
    Removing drv_memc.o(i.drv_memc_set_te_ind), (16 bytes).
    Removing drv_memc.o(i.drv_memc_set_tear_hwclr), (16 bytes).
    Removing drv_memc.o(i.drv_memc_set_vidc_fb_arb), (14 bytes).
    Removing drv_memc.o(i.drv_memc_set_write_trigger_line), (16 bytes).
    Removing drv_param_init.o(.rev16_text), (4 bytes).
    Removing drv_param_init.o(.revsh_text), (4 bytes).
    Removing drv_param_init.o(i.drv_param_init_set_scld_filter), (100 bytes).
    Removing drv_pwm.o(.rev16_text), (4 bytes).
    Removing drv_pwm.o(.revsh_text), (4 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_clear_pwm_int_all), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_enable), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_counter_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_current_count), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_high_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_low_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_register_callback), (24 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_set_pwm_int), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_set_sys_int), (52 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_get_sync_flag), (16 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_pause), (28 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_sync_mode), (32 bytes).
    Removing drv_rxbr.o(.rev16_text), (4 bytes).
    Removing drv_rxbr.o(.revsh_text), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_dsc_flush), (16 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_cur_hline_rcv_cnt), (8 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_ipi_vsync_interval), (8 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_pix_fmt), (8 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_col_addr), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_compress), (24 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_page_addr), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_soft_reset), (98 bytes).
    Removing drv_spi_dma.o(.rev16_text), (4 bytes).
    Removing drv_spi_dma.o(.revsh_text), (4 bytes).
    Removing drv_spi_dma.o(i.__NVIC_ClearPendingIRQ), (24 bytes).
    Removing drv_spi_dma.o(i.drv_spi_abort_dma), (108 bytes).
    Removing drv_spi_dma.o(i.drv_spi_dma_callback), (60 bytes).
    Removing drv_spi_dma.o(i.drv_spi_dma_ch6_init), (208 bytes).
    Removing drv_spi_dma.o(i.drv_spi_dma_init), (220 bytes).
    Removing drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback), (48 bytes).
    Removing drv_spi_dma.o(i.drv_spi_set_dma_irq_callback), (88 bytes).
    Removing drv_spi_dma.o(i.drv_spim_dma_read), (96 bytes).
    Removing drv_spi_dma.o(i.drv_spim_dma_write), (60 bytes).
    Removing drv_spi_dma.o(i.drv_spis_dma_write), (72 bytes).
    Removing drv_spi_dma.o(.bss), (480 bytes).
    Removing drv_spi_dma.o(.data), (16 bytes).
    Removing drv_swire.o(.rev16_text), (4 bytes).
    Removing drv_swire.o(.revsh_text), (4 bytes).
    Removing drv_swire.o(i.drv_swire_enable), (28 bytes).
    Removing drv_swire.o(i.drv_swire_register_callback), (12 bytes).
    Removing drv_swire.o(i.drv_swire_set_bit_time), (24 bytes).
    Removing drv_swire.o(i.drv_swire_set_pulse_count), (12 bytes).
    Removing drv_sys_cfg.o(.rev16_text), (4 bytes).
    Removing drv_sys_cfg.o(.revsh_text), (4 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_dma_req_mask), (32 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_read_version0_id), (12 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_set_ap_reset), (28 bytes).
    Removing drv_timer.o(.rev16_text), (4 bytes).
    Removing drv_timer.o(.revsh_text), (4 bytes).
    Removing drv_timer.o(i.drv_timer_clean_timer_value), (12 bytes).
    Removing drv_timer.o(i.drv_timer_get_current_count), (10 bytes).
    Removing drv_timer.o(i.drv_timer_get_match), (10 bytes).
    Removing drv_vidc.o(.rev16_text), (4 bytes).
    Removing drv_vidc.o(.revsh_text), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_clear_status0), (14 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_cap_pixel), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_signal_frame), (30 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_int_source), (38 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status0), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status1), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status2), (6 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_dsc_thresh), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_frmst_latency), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_inff_thresh), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_irq_line), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_module_enable), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_outff_thresh), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_update_src_format), (14 bytes).
    Removing irq_redirect .o(.rev16_text), (4 bytes).
    Removing irq_redirect .o(.revsh_text), (4 bytes).
    Removing drv_phy_common.o(.rev16_text), (4 bytes).
    Removing drv_phy_common.o(.revsh_text), (4 bytes).
    Removing drv_phy_common.o(i.drv_phy_get_calibration), (60 bytes).
    Removing drv_phy_common.o(.data), (1 bytes).
    Removing drv_pwr.o(.rev16_text), (4 bytes).
    Removing drv_pwr.o(.revsh_text), (4 bytes).
    Removing drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode), (44 bytes).
    Removing drv_i2c_master.o(.rev16_text), (4 bytes).
    Removing drv_i2c_master.o(.revsh_text), (4 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_bus_init), (36 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_disable_intr), (16 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_get_fifo_status), (28 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_read_data), (32 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_set_fifo_threshold), (24 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_set_sys_mask), (48 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_write_data), (32 bytes).
    Removing drv_i2c_slave.o(.rev16_text), (4 bytes).
    Removing drv_i2c_slave.o(.revsh_text), (4 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_bus_init), (36 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_disable_intr), (16 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_enable), (16 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_get_tx_byte_num), (12 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_read_data), (32 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_set_fifo_threshold), (24 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_set_sys_mask), (48 bytes).
    Removing drv_spi_master.o(.rev16_text), (4 bytes).
    Removing drv_spi_master.o(.revsh_text), (4 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_deinit), (40 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_disable_int), (68 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_enable_int), (72 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_enable_rx_dma), (32 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_enable_tx_dma), (28 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_get_dma_address), (8 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_gpio_init), (32 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_set_intr_callback), (12 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_switch_sclk), (28 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_write_data), (44 bytes).
    Removing drv_spi_master.o(i.drv_spi_master_init), (164 bytes).
    Removing drv_chip_info.o(.rev16_text), (4 bytes).
    Removing drv_chip_info.o(.revsh_text), (4 bytes).
    Removing drv_dsc_dec.o(.rev16_text), (4 bytes).
    Removing drv_dsc_dec.o(.revsh_text), (4 bytes).
    Removing drv_dsc_dec.o(i.drv_dsc_dec_set_u32_pps), (120 bytes).
    Removing hal_spi_slave.o(.rev16_text), (4 bytes).
    Removing hal_spi_slave.o(.revsh_text), (4 bytes).
    Removing hal_spi_slave.o(i.hal_spi_s_set_high_impedance), (100 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_auto_transfer_abort), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start), (56 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_busy), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_deinit), (10 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_disable), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_enable), (96 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_flush_fifo), (20 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_get_rxfifo_notempty), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_gpio_init), (8 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_init), (76 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_read_data), (10 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_register_callback), (12 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_reset_tx), (68 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_set_auto_rx_buffer), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_set_auto_tx_buffer), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_write_data), (14 bytes).
    Removing drv_fls_dma.o(.rev16_text), (4 bytes).
    Removing drv_fls_dma.o(.revsh_text), (4 bytes).
    Removing drv_fls_dma.o(i.fls_abort_dma), (42 bytes).
    Removing drv_fls_dma.o(i.fls_dma_disable), (10 bytes).
    Removing drv_fls_dma.o(i.fls_dma_enable), (10 bytes).
    Removing drv_fls_dma.o(i.fls_dma_read_prepare), (86 bytes).
    Removing drv_fls_dma.o(i.fls_dma_write_prepare), (82 bytes).
    Removing drv_fls_dma.o(i.fls_read_dmacallback), (32 bytes).
    Removing drv_fls_dma.o(i.fls_transfer_create_handle_dma), (208 bytes).
    Removing drv_fls_dma.o(i.fls_transfer_dma), (112 bytes).
    Removing drv_fls_dma.o(i.fls_transfer_get_receive_count_dma), (44 bytes).
    Removing drv_fls_dma.o(i.fls_write_dmacallback), (32 bytes).
    Removing drv_fls_dma.o(.data), (8 bytes).
    Removing drv_uart.o(.rev16_text), (4 bytes).
    Removing drv_uart.o(.revsh_text), (4 bytes).
    Removing drv_uart.o(i.UART_AbortReceive), (30 bytes).
    Removing drv_uart.o(i.UART_AbortSend), (30 bytes).
    Removing drv_uart.o(i.UART_Deinit), (28 bytes).
    Removing drv_uart.o(i.UART_Disable_IT), (68 bytes).
    Removing drv_uart.o(i.UART_EnableDma), (32 bytes).
    Removing drv_uart.o(i.UART_Enable_IT), (44 bytes).
    Removing drv_uart.o(i.UART_GetDefaultConfig), (72 bytes).
    Removing drv_uart.o(i.UART_GetFIFO_Ctrl), (20 bytes).
    Removing drv_uart.o(i.UART_GetReceiveCount), (22 bytes).
    Removing drv_uart.o(i.UART_GetReceiveStatus), (20 bytes).
    Removing drv_uart.o(i.UART_GetRxRingBufferLength), (28 bytes).
    Removing drv_uart.o(i.UART_GetSendCount), (22 bytes).
    Removing drv_uart.o(i.UART_GetSendStatus), (20 bytes).
    Removing drv_uart.o(i.UART_ReadBlocking), (32 bytes).
    Removing drv_uart.o(i.UART_ReceiveNonBlocking), (50 bytes).
    Removing drv_uart.o(i.UART_ResetTxFIFO), (36 bytes).
    Removing drv_uart.o(i.UART_SendNonBlocking), (38 bytes).
    Removing drv_uart.o(i.UART_TransferCreateHandle), (96 bytes).
    Removing drv_uart.o(i.UART_TransferStartRingBuffer), (30 bytes).
    Removing drv_uart.o(.constdata), (1 bytes).
    Removing drv_uart_dma.o(.rev16_text), (4 bytes).
    Removing drv_uart_dma.o(.revsh_text), (4 bytes).
    Removing drv_uart_dma.o(i.UART_DMAInit), (76 bytes).
    Removing drv_uart_dma.o(i.UART_TransferAbortReceiveDMA), (16 bytes).
    Removing drv_uart_dma.o(i.UART_TransferAbortSendDMA), (16 bytes).
    Removing drv_uart_dma.o(i.UART_TransferCreateHandleDMA), (176 bytes).
    Removing drv_uart_dma.o(i.UART_TransferGetReceiveCountDMA), (44 bytes).
    Removing drv_uart_dma.o(i.UART_TransferReceiveDMA), (68 bytes).
    Removing drv_uart_dma.o(i.UART_TransferReceiveDMACallback), (34 bytes).
    Removing drv_uart_dma.o(i.UART_TransferSendDMA), (68 bytes).
    Removing drv_uart_dma.o(i.UART_TransferSendDMACallback), (34 bytes).
    Removing drv_uart_dma.o(.data), (8 bytes).
    Removing drv_wdg.o(.rev16_text), (4 bytes).
    Removing drv_wdg.o(.revsh_text), (4 bytes).
    Removing drv_wdg.o(i.drv_wdg_clear_counter), (16 bytes).
    Removing drv_wdg.o(i.drv_wdg_enable), (32 bytes).
    Removing drv_wdg.o(i.drv_wdg_load_match), (12 bytes).
    Removing drv_wdg.o(i.drv_wdg_register_callback), (12 bytes).
    Removing drv_wdg.o(i.drv_wdg_sel_mode), (28 bytes).
    Removing drv_efuse.o(.rev16_text), (4 bytes).
    Removing drv_efuse.o(.revsh_text), (4 bytes).
    Removing drv_efuse.o(i.drv_efuse_crc_cal), (128 bytes).
    Removing drv_efuse.o(i.drv_efuse_get_default_config), (26 bytes).
    Removing drv_efuse.o(i.drv_efuse_int_disable), (12 bytes).
    Removing drv_efuse.o(i.drv_efuse_write), (46 bytes).
    Removing drv_efuse.o(i.drv_efuse_write_req), (22 bytes).
    Removing drv_spi_slave.o(.rev16_text), (4 bytes).
    Removing drv_spi_slave.o(.revsh_text), (4 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_deinit), (40 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_disable_int), (68 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_enable_int), (72 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_enable_rx_dma), (32 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_enable_tx_dma), (20 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_get_dma_address), (8 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_gpio_init), (24 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_read_data), (32 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_switch_sclk), (28 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_write_data), (44 bytes).
    Removing drv_spi_slave.o(i.drv_spi_slave_init), (76 bytes).
    Removing dflti.o(.text), (40 bytes).

588 unused section(s) (total 24377 bytes) removed from the image.

==============================================================================

Image Symbol Table

    Local Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    ../clib/../cmprslib/zerorunl2.c          0x00000000   Number         0  __dczerorl2.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  idiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uldiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uidiv.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry5.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry2.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11b.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llshl.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llushr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llsshr.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf1.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf0.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf8.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf6.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfb.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfa.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf2.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf3.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf4.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf7.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf5.o ABSOLUTE
    ../clib/microlib/printf/stubs.s          0x00000000   Number         0  stubs.o ABSOLUTE
    ../clib/microlib/stdio/streams.c         0x00000000   Number         0  stdout.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpyb.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpya.o ABSOLUTE
    ../clib/microlib/string/memset.c         0x00000000   Number         0  memseta.o ABSOLUTE
    ../clib/microlib/stubs.s                 0x00000000   Number         0  iusefp.o ABSOLUTE
    ../fplib/microlib/f2d.c                  0x00000000   Number         0  f2d.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  fadd.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  dadd.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  fdiv.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  ddiv.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  fepilogue.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  depilogue.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  ffixi.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixi.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixui.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  ffixui.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixul.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  fflti.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  dfltui.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  dflti.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  ffltui.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  dmul.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  fmul.o ABSOLUTE
    ../fplib/microlib/fpscalb.c              0x00000000   Number         0  fscalb.o ABSOLUTE
    ../mathlib/ceil.c                        0x00000000   Number         0  ceil.o ABSOLUTE
    ..\..\..\src\common\tau_delay.c          0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\..\..\src\common\tau_log.c            0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\..\..\src\driver\robin\src\drv_chip_info.c 0x00000000   Number         0  drv_chip_info.o ABSOLUTE
    ..\..\..\src\driver\robin\src\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_fls.c 0x00000000   Number         0  drv_fls.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_fls_dma.c 0x00000000   Number         0  drv_fls_dma.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_i2c_dma.c 0x00000000   Number         0  drv_i2c_dma.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_i2c_master.c 0x00000000   Number         0  drv_i2c_master.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_i2c_slave.c 0x00000000   Number         0  drv_i2c_slave.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_param_init.c 0x00000000   Number         0  drv_param_init.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_pwm.c 0x00000000   Number         0  drv_pwm.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_spi_dma.c 0x00000000   Number         0  drv_spi_dma.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_spi_master.c 0x00000000   Number         0  drv_spi_master.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_spi_slave.c 0x00000000   Number         0  drv_spi_slave.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_uart_dma.c 0x00000000   Number         0  drv_uart_dma.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_wdg.c 0x00000000   Number         0  drv_wdg.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\irq_redirect .c 0x00000000   Number         0  irq_redirect .o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\hal_i2c_master.c 0x00000000   Number         0  hal_i2c_master.o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\hal_i2c_slave.c 0x00000000   Number         0  hal_i2c_slave.o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\hal_pwm.c 0x00000000   Number         0  hal_pwm.o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\hal_spi_master.c 0x00000000   Number         0  hal_spi_master.o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\hal_spi_slave.c 0x00000000   Number         0  hal_spi_slave.o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\hal_swire.c 0x00000000   Number         0  hal_swire.o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\hal_timer.c 0x00000000   Number         0  hal_timer.o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\internal\dcs_packet_fifo.c 0x00000000   Number         0  dcs_packet_fifo.o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\internal\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\internal\norflash.c 0x00000000   Number         0  norflash.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_delay.c     0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_log.c       0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\\..\\..\\src\\driver\\robin\\src\\drv_chip_info.c 0x00000000   Number         0  drv_chip_info.o ABSOLUTE
    ..\\..\\..\\src\\driver\\robin\\src\\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_fls.c 0x00000000   Number         0  drv_fls.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_fls_dma.c 0x00000000   Number         0  drv_fls_dma.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_i2c_dma.c 0x00000000   Number         0  drv_i2c_dma.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_i2c_master.c 0x00000000   Number         0  drv_i2c_master.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_i2c_slave.c 0x00000000   Number         0  drv_i2c_slave.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_param_init.c 0x00000000   Number         0  drv_param_init.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_pwm.c 0x00000000   Number         0  drv_pwm.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_spi_dma.c 0x00000000   Number         0  drv_spi_dma.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_spi_master.c 0x00000000   Number         0  drv_spi_master.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_spi_slave.c 0x00000000   Number         0  drv_spi_slave.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_uart_dma.c 0x00000000   Number         0  drv_uart_dma.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_wdg.c 0x00000000   Number         0  drv_wdg.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\irq_redirect .c 0x00000000   Number         0  irq_redirect .o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\hal\\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\hal\\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\hal\\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\hal\\hal_i2c_master.c 0x00000000   Number         0  hal_i2c_master.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\hal\\hal_i2c_slave.c 0x00000000   Number         0  hal_i2c_slave.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\hal\\hal_pwm.c 0x00000000   Number         0  hal_pwm.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\hal\\hal_spi_master.c 0x00000000   Number         0  hal_spi_master.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\hal\\hal_spi_slave.c 0x00000000   Number         0  hal_spi_slave.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\hal\\hal_swire.c 0x00000000   Number         0  hal_swire.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\hal\\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\hal\\hal_timer.c 0x00000000   Number         0  hal_timer.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\hal\\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\hal\\internal\\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\hal\\internal\\norflash.c 0x00000000   Number         0  norflash.o ABSOLUTE
    ..\\src\\app\\demo\\ap_demo.c            0x00000000   Number         0  ap_demo.o ABSOLUTE
    ..\\src\\app\\demo\\app_tp_for_custom_s8.c 0x00000000   Number         0  app_tp_for_custom_s8.o ABSOLUTE
    ..\\src\\app\\demo\\app_tp_transfer.c    0x00000000   Number         0  app_tp_transfer.o ABSOLUTE
    ..\\src\\app\\main.c                     0x00000000   Number         0  main.o ABSOLUTE
    ..\\src\\board\\board.c                  0x00000000   Number         0  board.o ABSOLUTE
    ..\src\app\demo\ap_demo.c                0x00000000   Number         0  ap_demo.o ABSOLUTE
    ..\src\app\demo\app_tp_for_custom_s8.c   0x00000000   Number         0  app_tp_for_custom_s8.o ABSOLUTE
    ..\src\app\demo\app_tp_transfer.c        0x00000000   Number         0  app_tp_transfer.o ABSOLUTE
    ..\src\app\main.c                        0x00000000   Number         0  main.o ABSOLUTE
    ..\src\board\board.c                     0x00000000   Number         0  board.o ABSOLUTE
    ..\src\board\startup\startup_ARMCM0.s    0x00000000   Number         0  startup_armcm0.o ABSOLUTE
    cdrcmple.s                               0x00000000   Number         0  cdrcmple.o ABSOLUTE
    cfrcmple.s                               0x00000000   Number         0  cfrcmple.o ABSOLUTE
    dc.s                                     0x00000000   Number         0  dc.o ABSOLUTE
    handlers.s                               0x00000000   Number         0  handlers.o ABSOLUTE
    init.s                                   0x00000000   Number         0  init.o ABSOLUTE
    RESET                                    0x00010000   Section      192  startup_armcm0.o(RESET)
    .ARM.Collect$$$$00000000                 0x000100c0   Section        0  entry.o(.ARM.Collect$$$$00000000)
    .ARM.Collect$$$$00000001                 0x000100c0   Section        4  entry2.o(.ARM.Collect$$$$00000001)
    .ARM.Collect$$$$00000004                 0x000100c4   Section        4  entry5.o(.ARM.Collect$$$$00000004)
    .ARM.Collect$$$$00000008                 0x000100c8   Section        0  entry7b.o(.ARM.Collect$$$$00000008)
    .ARM.Collect$$$$0000000A                 0x000100c8   Section        0  entry8b.o(.ARM.Collect$$$$0000000A)
    .ARM.Collect$$$$0000000B                 0x000100c8   Section        8  entry9a.o(.ARM.Collect$$$$0000000B)
    .ARM.Collect$$$$0000000D                 0x000100d0   Section        0  entry10a.o(.ARM.Collect$$$$0000000D)
    .ARM.Collect$$$$0000000F                 0x000100d0   Section        0  entry11a.o(.ARM.Collect$$$$0000000F)
    .ARM.Collect$$$$00002712                 0x000100d0   Section        4  entry2.o(.ARM.Collect$$$$00002712)
    __lit__00000000                          0x000100d0   Data           4  entry2.o(.ARM.Collect$$$$00002712)
    .text                                    0x000100d4   Section      120  startup_armcm0.o(.text)
    .text                                    0x0001014c   Section        0  uidiv.o(.text)
    .text                                    0x00010178   Section        0  idiv.o(.text)
    .text                                    0x000101a0   Section        0  memcpya.o(.text)
    .text                                    0x000101c4   Section        0  memseta.o(.text)
    .text                                    0x000101e8   Section        0  fadd.o(.text)
    .text                                    0x0001029a   Section        0  fmul.o(.text)
    .text                                    0x00010314   Section        0  fdiv.o(.text)
    .text                                    0x00010390   Section        0  fscalb.o(.text)
    .text                                    0x000103a8   Section        0  dadd.o(.text)
    .text                                    0x0001050c   Section        0  dmul.o(.text)
    .text                                    0x000105dc   Section        0  ddiv.o(.text)
    .text                                    0x000106cc   Section        0  fflti.o(.text)
    .text                                    0x000106e2   Section        0  ffltui.o(.text)
    .text                                    0x000106f0   Section        0  dfltui.o(.text)
    .text                                    0x0001070c   Section        0  ffixi.o(.text)
    .text                                    0x0001073e   Section        0  ffixui.o(.text)
    .text                                    0x00010768   Section        0  dfixi.o(.text)
    .text                                    0x000107b0   Section        0  dfixui.o(.text)
    .text                                    0x000107ec   Section        0  f2d.o(.text)
    .text                                    0x00010814   Section       20  cfrcmple.o(.text)
    .text                                    0x00010828   Section        0  uldiv.o(.text)
    .text                                    0x00010888   Section        0  llshl.o(.text)
    .text                                    0x000108a8   Section        0  llushr.o(.text)
    .text                                    0x000108ca   Section        0  llsshr.o(.text)
    .text                                    0x000108f0   Section        0  fepilogue.o(.text)
    .text                                    0x000108f0   Section        0  iusefp.o(.text)
    .text                                    0x00010972   Section        0  depilogue.o(.text)
    .text                                    0x00010a30   Section        0  dfixul.o(.text)
    .text                                    0x00010a70   Section       40  cdrcmple.o(.text)
    .text                                    0x00010a98   Section       36  init.o(.text)
    .text                                    0x00010abc   Section        0  __dczerorl2.o(.text)
    i.ADC_IRQn_Handler                       0x00010b14   Section        0  irq_redirect .o(i.ADC_IRQn_Handler)
    i.AP_NRESET_IRQn_Handler                 0x00010b2c   Section        0  irq_redirect .o(i.AP_NRESET_IRQn_Handler)
    i.DMA_IRQn_Handler                       0x00010b44   Section        0  irq_redirect .o(i.DMA_IRQn_Handler)
    i.EXTI_INT0_IRQn_Handler                 0x00010b58   Section        0  irq_redirect .o(i.EXTI_INT0_IRQn_Handler)
    i.EXTI_INT1_IRQn_Handler                 0x00010b74   Section        0  irq_redirect .o(i.EXTI_INT1_IRQn_Handler)
    i.EXTI_INT2_IRQn_Handler                 0x00010b90   Section        0  irq_redirect .o(i.EXTI_INT2_IRQn_Handler)
    i.EXTI_INT3_IRQn_Handler                 0x00010bac   Section        0  irq_redirect .o(i.EXTI_INT3_IRQn_Handler)
    i.EXTI_INT4_IRQn_Handler                 0x00010bc8   Section        0  irq_redirect .o(i.EXTI_INT4_IRQn_Handler)
    i.EXTI_INT5_IRQn_Handler                 0x00010be4   Section        0  irq_redirect .o(i.EXTI_INT5_IRQn_Handler)
    i.EXTI_INT6_IRQn_Handler                 0x00010c00   Section        0  irq_redirect .o(i.EXTI_INT6_IRQn_Handler)
    i.EXTI_INT7_IRQn_Handler                 0x00010c1c   Section        0  irq_redirect .o(i.EXTI_INT7_IRQn_Handler)
    i.FLSCTRL_IRQn_Handler                   0x00010c38   Section        0  irq_redirect .o(i.FLSCTRL_IRQn_Handler)
    i.Gpio_swire_output                      0x00010c4c   Section        0  ap_demo.o(i.Gpio_swire_output)
    i.HardFault_Handler                      0x00010c9c   Section        0  irq_redirect .o(i.HardFault_Handler)
    i.I2C0_IRQn_Handler                      0x00010cb0   Section        0  irq_redirect .o(i.I2C0_IRQn_Handler)
    i.I2C1_IRQn_Handler                      0x00010cc8   Section        0  irq_redirect .o(i.I2C1_IRQn_Handler)
    i.LCDC_IRQn_Handler                      0x00010ce0   Section        0  irq_redirect .o(i.LCDC_IRQn_Handler)
    i.LOG_printf                             0x00010cf8   Section        0  tau_log.o(i.LOG_printf)
    i.MEMC_IRQn_Handler                      0x00010d20   Section        0  irq_redirect .o(i.MEMC_IRQn_Handler)
    i.MIPI_RX_IRQn_Handler                   0x00010d38   Section        0  irq_redirect .o(i.MIPI_RX_IRQn_Handler)
    i.MIPI_TX_IRQn_Handler                   0x00010d50   Section        0  irq_redirect .o(i.MIPI_TX_IRQn_Handler)
    i.PWMDET_IRQn_Handler                    0x00010d68   Section        0  irq_redirect .o(i.PWMDET_IRQn_Handler)
    i.PWM_Task                               0x00010d84   Section        0  ap_demo.o(i.PWM_Task)
    i.S20_Start_init                         0x00010e34   Section        0  app_tp_transfer.o(i.S20_Start_init)
    i.SPIM_IRQn_Handler                      0x00010f68   Section        0  irq_redirect .o(i.SPIM_IRQn_Handler)
    i.SPIS_IRQn_Handler                      0x00010f84   Section        0  irq_redirect .o(i.SPIS_IRQn_Handler)
    i.SWIRE_IRQn_Handler                     0x00010fa0   Section        0  irq_redirect .o(i.SWIRE_IRQn_Handler)
    i.SysTick_Handler                        0x00010fbc   Section        0  irq_redirect .o(i.SysTick_Handler)
    i.TIMER0_IRQn_Handler                    0x00010fd4   Section        0  irq_redirect .o(i.TIMER0_IRQn_Handler)
    i.UART_DisableDma                        0x00010fec   Section        0  drv_uart.o(i.UART_DisableDma)
    i.UART_GetInstance                       0x00010fee   Section        0  drv_uart.o(i.UART_GetInstance)
    i.__scatterload_copy                     0x00010ff2   Section       14  handlers.o(i.__scatterload_copy)
    .ARM.__at_0x11000                        0x00011000   Section       20  drv_common.o(.ARM.__at_0x11000)
    i.TIMER1_IRQn_Handler                    0x00011014   Section        0  irq_redirect .o(i.TIMER1_IRQn_Handler)
    i.TIMER2_IRQn_Handler                    0x0001102c   Section        0  irq_redirect .o(i.TIMER2_IRQn_Handler)
    i.TIMER3_IRQn_Handler                    0x00011044   Section        0  irq_redirect .o(i.TIMER3_IRQn_Handler)
    i.UART0_IRQ_Handle                       0x0001105c   Section        0  drv_uart.o(i.UART0_IRQ_Handle)
    i.UART_IRQn_Handler                      0x00011078   Section        0  irq_redirect .o(i.UART_IRQn_Handler)
    i.UART_ResetRxFIFO                       0x00011090   Section        0  drv_uart.o(i.UART_ResetRxFIFO)
    i.UART_SetBaudRate                       0x000110b4   Section        0  drv_uart.o(i.UART_SetBaudRate)
    i.UART_SwitchSCLK                        0x000110fc   Section        0  drv_uart.o(i.UART_SwitchSCLK)
    i.UART_TransferHandleIRQ                 0x00011116   Section        0  drv_uart.o(i.UART_TransferHandleIRQ)
    i.UART_WriteBlocking                     0x0001124a   Section        0  drv_uart.o(i.UART_WriteBlocking)
    i.UART_init                              0x00011264   Section        0  drv_uart.o(i.UART_init)
    i.VIDC_IRQn_Handler                      0x00011320   Section        0  irq_redirect .o(i.VIDC_IRQn_Handler)
    i.VPRE_IRQn_Handler                      0x00011338   Section        0  irq_redirect .o(i.VPRE_IRQn_Handler)
    i.WDG_IRQn_Handler                       0x00011350   Section        0  irq_redirect .o(i.WDG_IRQn_Handler)
    i.__0printf                              0x00011368   Section        0  printfa.o(i.__0printf)
    i.__0vsprintf                            0x00011388   Section        0  printfa.o(i.__0vsprintf)
    i.__ARM_clz                              0x000113ac   Section        0  depilogue.o(i.__ARM_clz)
    i.__ARM_common_switch8                   0x000113da   Section        0  hal_dsi_rx_ctrl.o(i.__ARM_common_switch8)
    i.__NVIC_ClearPendingIRQ                 0x000113f4   Section        0  drv_i2c_master.o(i.__NVIC_ClearPendingIRQ)
    __NVIC_ClearPendingIRQ                   0x000113f5   Thumb Code    18  drv_i2c_master.o(i.__NVIC_ClearPendingIRQ)
    i.__NVIC_ClearPendingIRQ                 0x0001140c   Section        0  drv_i2c_slave.o(i.__NVIC_ClearPendingIRQ)
    __NVIC_ClearPendingIRQ                   0x0001140d   Thumb Code    18  drv_i2c_slave.o(i.__NVIC_ClearPendingIRQ)
    i.__NVIC_ClearPendingIRQ                 0x00011424   Section        0  drv_spi_master.o(i.__NVIC_ClearPendingIRQ)
    __NVIC_ClearPendingIRQ                   0x00011425   Thumb Code    18  drv_spi_master.o(i.__NVIC_ClearPendingIRQ)
    i.__NVIC_DisableIRQ                      0x0001143c   Section        0  drv_rxbr.o(i.__NVIC_DisableIRQ)
    __NVIC_DisableIRQ                        0x0001143d   Thumb Code    26  drv_rxbr.o(i.__NVIC_DisableIRQ)
    i.__NVIC_EnableIRQ                       0x0001145c   Section        0  drv_rxbr.o(i.__NVIC_EnableIRQ)
    __NVIC_EnableIRQ                         0x0001145d   Thumb Code    18  drv_rxbr.o(i.__NVIC_EnableIRQ)
    i.__NVIC_SetPriority                     0x00011474   Section        0  hal_spi_slave.o(i.__NVIC_SetPriority)
    __NVIC_SetPriority                       0x00011475   Thumb Code    60  hal_spi_slave.o(i.__NVIC_SetPriority)
    i.__scatterload_null                     0x000114b8   Section        2  handlers.o(i.__scatterload_null)
    i.__scatterload_zeroinit                 0x000114ba   Section       14  handlers.o(i.__scatterload_zeroinit)
    i._fp_digits                             0x000114c8   Section        0  printfa.o(i._fp_digits)
    _fp_digits                               0x000114c9   Thumb Code   344  printfa.o(i._fp_digits)
    i._printf_core                           0x0001163c   Section        0  printfa.o(i._printf_core)
    _printf_core                             0x0001163d   Thumb Code  1754  printfa.o(i._printf_core)
    i._printf_post_padding                   0x00011d28   Section        0  printfa.o(i._printf_post_padding)
    _printf_post_padding                     0x00011d29   Thumb Code    32  printfa.o(i._printf_post_padding)
    i._printf_pre_padding                    0x00011d48   Section        0  printfa.o(i._printf_pre_padding)
    _printf_pre_padding                      0x00011d49   Thumb Code    44  printfa.o(i._printf_pre_padding)
    i._sputc                                 0x00011d74   Section        0  printfa.o(i._sputc)
    _sputc                                   0x00011d75   Thumb Code    10  printfa.o(i._sputc)
    i.ap_dcs_read                            0x00011d80   Section        0  ap_demo.o(i.ap_dcs_read)
    ap_dcs_read                              0x00011d81   Thumb Code  4446  ap_demo.o(i.ap_dcs_read)
    i.ap_demo                                0x00012f04   Section        0  ap_demo.o(i.ap_demo)
    i.ap_get_reg_ca                          0x000130b0   Section        0  ap_demo.o(i.ap_get_reg_ca)
    ap_get_reg_ca                            0x000130b1   Thumb Code    18  ap_demo.o(i.ap_get_reg_ca)
    i.ap_get_reg_df                          0x000130c8   Section        0  ap_demo.o(i.ap_get_reg_df)
    ap_get_reg_df                            0x000130c9   Thumb Code   134  ap_demo.o(i.ap_get_reg_df)
    i.ap_reset_cb                            0x00013154   Section        0  ap_demo.o(i.ap_reset_cb)
    ap_reset_cb                              0x00013155   Thumb Code    40  ap_demo.o(i.ap_reset_cb)
    i.ap_set_backlight                       0x000131b8   Section        0  ap_demo.o(i.ap_set_backlight)
    ap_set_backlight                         0x000131b9   Thumb Code   206  ap_demo.o(i.ap_set_backlight)
    i.ap_set_display_off                     0x00013298   Section        0  ap_demo.o(i.ap_set_display_off)
    ap_set_display_off                       0x00013299   Thumb Code    50  ap_demo.o(i.ap_set_display_off)
    i.ap_set_display_on                      0x000132f0   Section        0  ap_demo.o(i.ap_set_display_on)
    ap_set_display_on                        0x000132f1   Thumb Code    18  ap_demo.o(i.ap_set_display_on)
    i.ap_set_enter_sleep_mode                0x00013328   Section        0  ap_demo.o(i.ap_set_enter_sleep_mode)
    ap_set_enter_sleep_mode                  0x00013329   Thumb Code    84  ap_demo.o(i.ap_set_enter_sleep_mode)
    i.ap_set_exit_sleep_mode                 0x000133b0   Section        0  ap_demo.o(i.ap_set_exit_sleep_mode)
    ap_set_exit_sleep_mode                   0x000133b1   Thumb Code    20  ap_demo.o(i.ap_set_exit_sleep_mode)
    i.ap_set_tp_calibration_04               0x000133f8   Section        0  ap_demo.o(i.ap_set_tp_calibration_04)
    ap_set_tp_calibration_04                 0x000133f9   Thumb Code    22  ap_demo.o(i.ap_set_tp_calibration_04)
    i.ap_tp_calibration                      0x00013414   Section        0  app_tp_transfer.o(i.ap_tp_calibration)
    i.app_ADC_IRQn_Handler                   0x000134c4   Section        0  drv_rxbr.o(i.app_ADC_IRQn_Handler)
    i.app_AP_NRESET_IRQn_Handler             0x000134e0   Section        0  drv_gpio.o(i.app_AP_NRESET_IRQn_Handler)
    i.app_EXTI_INT0_IRQn_Handler             0x00013504   Section        0  drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler)
    i.app_EXTI_INT1_IRQn_Handler             0x00013520   Section        0  drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler)
    i.app_EXTI_INT2_IRQn_Handler             0x0001353c   Section        0  drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler)
    i.app_EXTI_INT3_IRQn_Handler             0x00013558   Section        0  drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler)
    i.app_EXTI_INT4_IRQn_Handler             0x00013574   Section        0  drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler)
    i.app_EXTI_INT5_IRQn_Handler             0x00013590   Section        0  drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler)
    i.app_EXTI_INT6_IRQn_Handler             0x000135ac   Section        0  drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler)
    i.app_EXTI_INT7_IRQn_Handler             0x000135c8   Section        0  drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler)
    i.app_HardFault_Handler                  0x000135e4   Section        0  drv_common.o(i.app_HardFault_Handler)
    i.app_I2C0_IRQn_Handler                  0x0001362c   Section        0  drv_i2c_slave.o(i.app_I2C0_IRQn_Handler)
    i.app_I2C1_IRQn_Handler                  0x0001363c   Section        0  drv_i2c_master.o(i.app_I2C1_IRQn_Handler)
    i.app_LCDC_IRQn_Handler                  0x0001364c   Section        0  hal_internal_vsync.o(i.app_LCDC_IRQn_Handler)
    i.app_MEMC_IRQn_Handler                  0x0001372c   Section        0  drv_memc.o(i.app_MEMC_IRQn_Handler)
    i.app_MIPI_RX_IRQn_Handler               0x000137b4   Section        0  drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler)
    i.app_MIPI_TX_IRQn_Handler               0x00013a40   Section        0  drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler)
    i.app_PWMDET_IRQn_Handler                0x00013ae0   Section        0  drv_pwm.o(i.app_PWMDET_IRQn_Handler)
    i.app_SPIM_IRQn_Handler                  0x00013b28   Section        0  drv_spi_master.o(i.app_SPIM_IRQn_Handler)
    i.app_SPIS_IRQn_Handler                  0x00013b58   Section        0  hal_spi_slave.o(i.app_SPIS_IRQn_Handler)
    i.app_SWIRE_IRQn_Handler                 0x00013bfc   Section        0  drv_swire.o(i.app_SWIRE_IRQn_Handler)
    i.app_SysTick_Handler                    0x00013c1c   Section        0  drv_common.o(i.app_SysTick_Handler)
    i.app_TIMER0_IRQn_Handler                0x00013c34   Section        0  drv_timer.o(i.app_TIMER0_IRQn_Handler)
    i.app_TIMER1_IRQn_Handler                0x00013c58   Section        0  drv_timer.o(i.app_TIMER1_IRQn_Handler)
    i.app_TIMER2_IRQn_Handler                0x00013c7c   Section        0  drv_timer.o(i.app_TIMER2_IRQn_Handler)
    i.app_TIMER3_IRQn_Handler                0x00013ca0   Section        0  drv_timer.o(i.app_TIMER3_IRQn_Handler)
    i.app_UART_IRQn_Handler                  0x00013cd4   Section        0  drv_uart.o(i.app_UART_IRQn_Handler)
    i.app_VIDC_IRQn_Handler                  0x00013cdc   Section        0  drv_vidc.o(i.app_VIDC_IRQn_Handler)
    i.app_VPRE_IRQn_Handler                  0x00013cf8   Section        0  drv_rxbr.o(i.app_VPRE_IRQn_Handler)
    i.app_WDG_IRQn_Handler                   0x00013d14   Section        0  drv_wdg.o(i.app_WDG_IRQn_Handler)
    i.app_dma_irq_handler                    0x00013d40   Section        0  drv_dma.o(i.app_dma_irq_handler)
    i.app_fls_ctrl_Handler                   0x00013d50   Section        0  norflash.o(i.app_fls_ctrl_Handler)
    i.app_tp_I2C_init                        0x00013d80   Section        0  app_tp_transfer.o(i.app_tp_I2C_init)
    i.app_tp_calibration_exec                0x00013da4   Section        0  ap_demo.o(i.app_tp_calibration_exec)
    i.app_tp_i2cs_callback                   0x00013e00   Section        0  app_tp_transfer.o(i.app_tp_i2cs_callback)
    app_tp_i2cs_callback                     0x00013e01   Thumb Code    42  app_tp_transfer.o(i.app_tp_i2cs_callback)
    i.app_tp_init                            0x00013e30   Section        0  app_tp_transfer.o(i.app_tp_init)
    i.app_tp_m_read                          0x00013e78   Section        0  app_tp_transfer.o(i.app_tp_m_read)
    app_tp_m_read                            0x00013e79   Thumb Code    32  app_tp_transfer.o(i.app_tp_m_read)
    i.app_tp_m_write                         0x00013e98   Section        0  app_tp_transfer.o(i.app_tp_m_write)
    app_tp_m_write                           0x00013e99   Thumb Code     8  app_tp_transfer.o(i.app_tp_m_write)
    i.app_tp_phone_analysis_data             0x00013ea0   Section        0  app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data)
    i.app_tp_phone_clear_reset_on            0x000141b8   Section        0  app_tp_transfer.o(i.app_tp_phone_clear_reset_on)
    i.app_tp_s_read                          0x000141c4   Section        0  app_tp_transfer.o(i.app_tp_s_read)
    i.app_tp_s_write                         0x000141cc   Section        0  app_tp_transfer.o(i.app_tp_s_write)
    i.app_tp_screen_analysis_int             0x000141d4   Section        0  app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int)
    i.app_tp_screen_init                     0x00014470   Section        0  app_tp_transfer.o(i.app_tp_screen_init)
    i.app_tp_screen_int_callback             0x000144a0   Section        0  app_tp_transfer.o(i.app_tp_screen_int_callback)
    app_tp_screen_int_callback               0x000144a1   Thumb Code     8  app_tp_transfer.o(i.app_tp_screen_int_callback)
    i.app_tp_transfer_screen_const           0x000144ac   Section        0  app_tp_transfer.o(i.app_tp_transfer_screen_const)
    app_tp_transfer_screen_const             0x000144ad   Thumb Code    50  app_tp_transfer.o(i.app_tp_transfer_screen_const)
    i.app_tp_transfer_screen_int             0x000144ec   Section        0  app_tp_transfer.o(i.app_tp_transfer_screen_int)
    i.app_tp_transfer_screen_start           0x000145d8   Section        0  app_tp_transfer.o(i.app_tp_transfer_screen_start)
    i.board_Init                             0x000145f0   Section        0  board.o(i.board_Init)
    i.calc_framebuffer_setting               0x0001460c   Section        0  hal_internal_vsync.o(i.calc_framebuffer_setting)
    calc_framebuffer_setting                 0x0001460d   Thumb Code   628  hal_internal_vsync.o(i.calc_framebuffer_setting)
    i.ceil                                   0x000148c0   Section        0  ceil.o(i.ceil)
    i.check_mipi_rx_tx_video_info            0x00014988   Section        0  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    check_mipi_rx_tx_video_info              0x00014989   Thumb Code    44  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    i.check_pkt_buf_rev                      0x000149b4   Section        0  hal_internal_vsync.o(i.check_pkt_buf_rev)
    check_pkt_buf_rev                        0x000149b5   Thumb Code    92  hal_internal_vsync.o(i.check_pkt_buf_rev)
    i.dcs_packet_fifo_alloc                  0x00014a44   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    i.dcs_packet_fifo_init                   0x00014a9c   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    i.dcs_packet_free_fifo_header            0x00014ab4   Section        0  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    i.dcs_packet_get_fifo_header             0x00014af8   Section        0  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    i.dcs_sw_filter                          0x00014b1c   Section        0  hal_internal_vsync.o(i.dcs_sw_filter)
    dcs_sw_filter                            0x00014b1d   Thumb Code    24  hal_internal_vsync.o(i.dcs_sw_filter)
    i.delayMs                                0x00014b38   Section        0  tau_delay.o(i.delayMs)
    i.delayUs                                0x00014b50   Section        0  tau_delay.o(i.delayUs)
    i.drv_ap_rst_trig_edge_detect            0x00014b74   Section        0  drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect)
    i.drv_chip_info_get_info                 0x00014bac   Section        0  drv_chip_info.o(i.drv_chip_info_get_info)
    i.drv_chip_info_init                     0x00014bb8   Section        0  drv_chip_info.o(i.drv_chip_info_init)
    i.drv_chip_rx_info_check                 0x00014bf8   Section        0  drv_chip_info.o(i.drv_chip_rx_info_check)
    i.drv_chip_rx_init_done                  0x00014cc0   Section        0  drv_chip_info.o(i.drv_chip_rx_init_done)
    i.drv_common_enable_systick              0x00014cd4   Section        0  drv_common.o(i.drv_common_enable_systick)
    i.drv_common_system_init                 0x00014d2c   Section        0  drv_common.o(i.drv_common_system_init)
    i.drv_crgu_clear_all_reset_flags         0x00014d34   Section        0  drv_crgu.o(i.drv_crgu_clear_all_reset_flags)
    i.drv_crgu_config_reset_modules          0x00014d40   Section        0  drv_crgu.o(i.drv_crgu_config_reset_modules)
    i.drv_crgu_set_ahb_pre_div               0x00014d50   Section        0  drv_crgu.o(i.drv_crgu_set_ahb_pre_div)
    i.drv_crgu_set_ahb_src                   0x00014d64   Section        0  drv_crgu.o(i.drv_crgu_set_ahb_src)
    i.drv_crgu_set_clock                     0x00014d78   Section        0  drv_crgu.o(i.drv_crgu_set_clock)
    i.drv_crgu_set_dpi_mux_src               0x00014d98   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_mux_src)
    i.drv_crgu_set_dpi_pre_div               0x00014dac   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_pre_div)
    i.drv_crgu_set_dpi_pre_src               0x00014dc4   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_pre_src)
    i.drv_crgu_set_dsc_core_div              0x00014dd8   Section        0  drv_crgu.o(i.drv_crgu_set_dsc_core_div)
    i.drv_crgu_set_dsco_src                  0x00014dec   Section        0  drv_crgu.o(i.drv_crgu_set_dsco_src)
    i.drv_crgu_set_dsco_src_div              0x00014e00   Section        0  drv_crgu.o(i.drv_crgu_set_dsco_src_div)
    i.drv_crgu_set_fb_div                    0x00014e14   Section        0  drv_crgu.o(i.drv_crgu_set_fb_div)
    i.drv_crgu_set_fb_src                    0x00014e28   Section        0  drv_crgu.o(i.drv_crgu_set_fb_src)
    i.drv_crgu_set_lcdc_div                  0x00014e3c   Section        0  drv_crgu.o(i.drv_crgu_set_lcdc_div)
    i.drv_crgu_set_lcdc_src                  0x00014e50   Section        0  drv_crgu.o(i.drv_crgu_set_lcdc_src)
    i.drv_crgu_set_mipi_cfg_src              0x00014e64   Section        0  drv_crgu.o(i.drv_crgu_set_mipi_cfg_src)
    i.drv_crgu_set_mipi_ref_src              0x00014e78   Section        0  drv_crgu.o(i.drv_crgu_set_mipi_ref_src)
    i.drv_crgu_set_reset                     0x00014e90   Section        0  drv_crgu.o(i.drv_crgu_set_reset)
    i.drv_crgu_set_rxbr_div                  0x00014ea8   Section        0  drv_crgu.o(i.drv_crgu_set_rxbr_div)
    i.drv_crgu_set_rxbr_src                  0x00014ebc   Section        0  drv_crgu.o(i.drv_crgu_set_rxbr_src)
    i.drv_crgu_set_vidc_src                  0x00014ed0   Section        0  drv_crgu.o(i.drv_crgu_set_vidc_src)
    i.drv_dma_clear_flag                     0x00014ee4   Section        0  drv_dma.o(i.drv_dma_clear_flag)
    i.drv_dma_create_handle                  0x00014efc   Section        0  drv_dma.o(i.drv_dma_create_handle)
    i.drv_dma_disenable_channel              0x00014f18   Section        0  drv_dma.o(i.drv_dma_disenable_channel)
    i.drv_dma_enable_channel                 0x00014f28   Section        0  drv_dma.o(i.drv_dma_enable_channel)
    i.drv_dma_enable_channel_interrupts      0x00014f38   Section        0  drv_dma.o(i.drv_dma_enable_channel_interrupts)
    i.drv_dma_get_channel_flag               0x00014f5c   Section        0  drv_dma.o(i.drv_dma_get_channel_flag)
    i.drv_dma_irq_handler                    0x00014f68   Section        0  drv_dma.o(i.drv_dma_irq_handler)
    i.drv_dma_prepar_transfer                0x00014ff8   Section        0  drv_dma.o(i.drv_dma_prepar_transfer)
    i.drv_dma_set_burst                      0x0001500a   Section        0  drv_dma.o(i.drv_dma_set_burst)
    i.drv_dma_set_callback                   0x00015024   Section        0  drv_dma.o(i.drv_dma_set_callback)
    i.drv_dma_set_transfer                   0x0001502c   Section        0  drv_dma.o(i.drv_dma_set_transfer)
    i.drv_dsc_dec_convert_pps_rc_parameter   0x00015070   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter)
    i.drv_dsc_dec_disable                    0x000150a6   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    i.drv_dsc_dec_enable                     0x000150b4   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    i.drv_dsc_dec_get_nslc                   0x00015128   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    i.drv_dsc_dec_set_u8_pps                 0x00015132   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps)
    i.drv_dsi_rx_calc_ipi_tx_delay           0x0001515c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    i.drv_dsi_rx_enable_irq                  0x00015260   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    i.drv_dsi_rx_get_color_bpp               0x000152a0   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    drv_dsi_rx_get_color_bpp                 0x000152a1   Thumb Code    62  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    i.drv_dsi_rx_get_color_pcc               0x000152f0   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    drv_dsi_rx_get_color_pcc                 0x000152f1   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    i.drv_dsi_rx_get_compression_en          0x0001530c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    i.drv_dsi_rx_get_max_ret_size            0x00015314   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size)
    i.drv_dsi_rx_power_up                    0x0001531a   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    i.drv_dsi_rx_set_ctrl_cfg                0x00015328   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    i.drv_dsi_rx_set_ddi_cfg                 0x00015348   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    i.drv_dsi_rx_set_inten                   0x00015358   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    i.drv_dsi_rx_set_ipi_cfg                 0x0001535c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    i.drv_dsi_rx_set_lane_swap               0x0001536c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    i.drv_dsi_rx_set_up_phy                  0x000153b4   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    i.drv_dsi_rx_shut_down                   0x00015484   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    i.drv_dsi_tx_command_header              0x00015492   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    i.drv_dsi_tx_command_mode_cfg            0x000154a6   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    i.drv_dsi_tx_command_put_payload         0x00015512   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    i.drv_dsi_tx_config_eotp                 0x00015516   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    i.drv_dsi_tx_config_int                  0x0001552e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    i.drv_dsi_tx_dpi_lpcmd_time              0x00015536   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    i.drv_dsi_tx_dpi_mode                    0x0001553e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    i.drv_dsi_tx_dpi_polarity                0x00015548   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    i.drv_dsi_tx_edpi_cmd_size               0x0001556c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    i.drv_dsi_tx_get_cmd_status              0x00015570   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    i.drv_dsi_tx_mode                        0x00015574   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    i.drv_dsi_tx_phy_clock_lane_auto_lp      0x00015578   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    i.drv_dsi_tx_phy_clock_lane_req_hs       0x00015590   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    i.drv_dsi_tx_phy_lane_mode               0x000155aa   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    i.drv_dsi_tx_phy_status_ready            0x000155b6   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    i.drv_dsi_tx_phy_status_stopstate        0x0001561a   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    i.drv_dsi_tx_phy_time_cfg                0x00015658   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    i.drv_dsi_tx_powerup                     0x00015676   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    i.drv_dsi_tx_response_mode               0x0001567e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    i.drv_dsi_tx_set_bta_ack                 0x0001569a   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    i.drv_dsi_tx_set_esc_div                 0x000156b2   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    i.drv_dsi_tx_set_int                     0x000156c0   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    i.drv_dsi_tx_set_time_out_div            0x000156f4   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    i.drv_dsi_tx_set_video_chunk             0x00015704   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    i.drv_dsi_tx_set_video_timing            0x0001570c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    i.drv_dsi_tx_shutdown                    0x0001572e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    i.drv_dsi_tx_timeout_cfg                 0x00015736   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    i.drv_dsi_tx_video_mode_cfg              0x0001575c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    i.drv_dsi_tx_video_mode_disable_hact_cmd 0x00015806   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_disable_hact_cmd)
    i.drv_dsi_tx_video_mode_set_lp_cmd       0x0001581c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd)
    i.drv_efuse_enter_inactive               0x00015834   Section        0  drv_efuse.o(i.drv_efuse_enter_inactive)
    i.drv_efuse_int_enable                   0x00015854   Section        0  drv_efuse.o(i.drv_efuse_int_enable)
    i.drv_efuse_read                         0x00015860   Section        0  drv_efuse.o(i.drv_efuse_read)
    i.drv_efuse_read_req                     0x00015892   Section        0  drv_efuse.o(i.drv_efuse_read_req)
    i.drv_gpio_get_input_data                0x000158ac   Section        0  drv_gpio.o(i.drv_gpio_get_input_data)
    i.drv_gpio_register_ap_reset_callback    0x000158c4   Section        0  drv_gpio.o(i.drv_gpio_register_ap_reset_callback)
    i.drv_gpio_register_callback             0x000158d0   Section        0  drv_gpio.o(i.drv_gpio_register_callback)
    i.drv_gpio_set_int                       0x000158e4   Section        0  drv_gpio.o(i.drv_gpio_set_int)
    i.drv_gpio_set_ioe                       0x00015928   Section        0  drv_gpio.o(i.drv_gpio_set_ioe)
    i.drv_gpio_set_mode0                     0x00015948   Section        0  drv_gpio.o(i.drv_gpio_set_mode0)
    i.drv_gpio_set_mode1                     0x00015958   Section        0  drv_gpio.o(i.drv_gpio_set_mode1)
    i.drv_gpio_set_mode2                     0x00015968   Section        0  drv_gpio.o(i.drv_gpio_set_mode2)
    i.drv_gpio_set_mode3                     0x00015978   Section        0  drv_gpio.o(i.drv_gpio_set_mode3)
    i.drv_gpio_set_output_data               0x00015988   Section        0  hal_gpio.o(i.drv_gpio_set_output_data)
    drv_gpio_set_output_data                 0x00015989   Thumb Code    26  hal_gpio.o(i.drv_gpio_set_output_data)
    i.drv_gpio_set_pull_state                0x000159a8   Section        0  drv_gpio.o(i.drv_gpio_set_pull_state)
    i.drv_i2c_dma_callback                   0x00015ad8   Section        0  drv_i2c_dma.o(i.drv_i2c_dma_callback)
    drv_i2c_dma_callback                     0x00015ad9   Thumb Code    40  drv_i2c_dma.o(i.drv_i2c_dma_callback)
    i.drv_i2c_dma_init                       0x00015b0c   Section        0  drv_i2c_dma.o(i.drv_i2c_dma_init)
    i.drv_i2c_enable_rx_dma                  0x00015bb8   Section        0  drv_i2c_dma.o(i.drv_i2c_enable_rx_dma)
    i.drv_i2c_enable_tx_dma                  0x00015bd2   Section        0  drv_i2c_dma.o(i.drv_i2c_enable_tx_dma)
    i.drv_i2c_m_clear_it_pending_bit         0x00015bec   Section        0  drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit)
    i.drv_i2c_m_enable                       0x00015c4c   Section        0  drv_i2c_master.o(i.drv_i2c_m_enable)
    i.drv_i2c_m_enable_intr                  0x00015c5c   Section        0  drv_i2c_master.o(i.drv_i2c_m_enable_intr)
    i.drv_i2c_m_set_callback                 0x00015c94   Section        0  drv_i2c_master.o(i.drv_i2c_m_set_callback)
    i.drv_i2c_master_init                    0x00015ca0   Section        0  drv_i2c_master.o(i.drv_i2c_master_init)
    i.drv_i2c_master_read_dma                0x00015d2c   Section        0  drv_i2c_dma.o(i.drv_i2c_master_read_dma)
    i.drv_i2c_master_write_dma               0x00015d88   Section        0  drv_i2c_dma.o(i.drv_i2c_master_write_dma)
    i.drv_i2c_master_write_read_cmd          0x00015dc4   Section        0  drv_i2c_dma.o(i.drv_i2c_master_write_read_cmd)
    drv_i2c_master_write_read_cmd            0x00015dc5   Thumb Code    46  drv_i2c_dma.o(i.drv_i2c_master_write_read_cmd)
    i.drv_i2c_s_clear_it_pending_bit         0x00015df4   Section        0  drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit)
    i.drv_i2c_s_enable_intr                  0x00015e50   Section        0  drv_i2c_slave.o(i.drv_i2c_s_enable_intr)
    i.drv_i2c_s_get_fifo_status              0x00015e84   Section        0  drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status)
    i.drv_i2c_s_set_callback                 0x00015ea0   Section        0  drv_i2c_slave.o(i.drv_i2c_s_set_callback)
    i.drv_i2c_s_write_data                   0x00015eac   Section        0  drv_i2c_slave.o(i.drv_i2c_s_write_data)
    i.drv_i2c_set_dma_irq_callback           0x00015ecc   Section        0  drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback)
    i.drv_i2c_slave_init                     0x00015f24   Section        0  drv_i2c_slave.o(i.drv_i2c_slave_init)
    i.drv_i2c_slave_write_dma                0x00015f68   Section        0  drv_i2c_dma.o(i.drv_i2c_slave_write_dma)
    i.drv_lcdc_config_bypass                 0x00015f84   Section        0  drv_lcdc.o(i.drv_lcdc_config_bypass)
    i.drv_lcdc_config_ccm                    0x00015f9c   Section        0  drv_lcdc.o(i.drv_lcdc_config_ccm)
    i.drv_lcdc_config_disp_mode              0x00015fcc   Section        0  drv_lcdc.o(i.drv_lcdc_config_disp_mode)
    i.drv_lcdc_config_dpi_polarity           0x00015fe2   Section        0  drv_lcdc.o(i.drv_lcdc_config_dpi_polarity)
    i.drv_lcdc_config_dpi_timing             0x00016006   Section        0  drv_lcdc.o(i.drv_lcdc_config_dpi_timing)
    i.drv_lcdc_config_edpi_mode              0x0001602c   Section        0  drv_lcdc.o(i.drv_lcdc_config_edpi_mode)
    i.drv_lcdc_config_endianness             0x00016042   Section        0  drv_lcdc.o(i.drv_lcdc_config_endianness)
    i.drv_lcdc_config_input_size             0x00016058   Section        0  drv_lcdc.o(i.drv_lcdc_config_input_size)
    i.drv_lcdc_config_int                    0x00016064   Section        0  drv_lcdc.o(i.drv_lcdc_config_int)
    i.drv_lcdc_config_int_single             0x00016082   Section        0  drv_lcdc.o(i.drv_lcdc_config_int_single)
    i.drv_lcdc_config_overwrite              0x000160a4   Section        0  drv_lcdc.o(i.drv_lcdc_config_overwrite)
    i.drv_lcdc_config_overwrite_rgb          0x000160c6   Section        0  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    i.drv_lcdc_config_partial_display_area   0x000160d2   Section        0  drv_lcdc.o(i.drv_lcdc_config_partial_display_area)
    i.drv_lcdc_config_partial_display_enable 0x000160ec   Section        0  drv_lcdc.o(i.drv_lcdc_config_partial_display_enable)
    i.drv_lcdc_config_scale_up_coef          0x0001610e   Section        0  drv_lcdc.o(i.drv_lcdc_config_scale_up_coef)
    i.drv_lcdc_config_scale_up_step          0x00016136   Section        0  drv_lcdc.o(i.drv_lcdc_config_scale_up_step)
    i.drv_lcdc_config_src_parameter          0x00016142   Section        0  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    i.drv_lcdc_config_thresh                 0x0001618e   Section        0  drv_lcdc.o(i.drv_lcdc_config_thresh)
    i.drv_lcdc_ctrl_flow                     0x00016194   Section        0  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    i.drv_lcdc_enable_shadow_reg             0x000161a6   Section        0  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    i.drv_lcdc_set_int                       0x000161c8   Section        0  drv_lcdc.o(i.drv_lcdc_set_int)
    i.drv_lcdc_set_video_hw_mode             0x000161fc   Section        0  drv_lcdc.o(i.drv_lcdc_set_video_hw_mode)
    i.drv_lcdc_start                         0x00016210   Section        0  drv_lcdc.o(i.drv_lcdc_start)
    i.drv_memc_clear_status                  0x00016230   Section        0  drv_memc.o(i.drv_memc_clear_status)
    i.drv_memc_enable_irq                    0x0001623c   Section        0  drv_memc.o(i.drv_memc_enable_irq)
    i.drv_memc_gen_a_tear_signal             0x0001627c   Section        0  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    i.drv_memc_get_status                    0x00016288   Section        0  drv_memc.o(i.drv_memc_get_status)
    i.drv_memc_rate_transfer_sel             0x0001629a   Section        0  drv_memc.o(i.drv_memc_rate_transfer_sel)
    i.drv_memc_sel_vsync                     0x000162aa   Section        0  drv_memc.o(i.drv_memc_sel_vsync)
    i.drv_memc_set_active_height             0x000162b8   Section        0  drv_memc.o(i.drv_memc_set_active_height)
    i.drv_memc_set_data_mode                 0x000162cc   Section        0  drv_memc.o(i.drv_memc_set_data_mode)
    i.drv_memc_set_double_buffer             0x000162d8   Section        0  drv_memc.o(i.drv_memc_set_double_buffer)
    i.drv_memc_set_double_buffer_reverse     0x000162e8   Section        0  drv_memc.o(i.drv_memc_set_double_buffer_reverse)
    i.drv_memc_set_fs_en_conditions          0x000162fa   Section        0  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    i.drv_memc_set_inten                     0x0001630a   Section        0  drv_memc.o(i.drv_memc_set_inten)
    i.drv_memc_set_lcdc_st_conditions        0x00016320   Section        0  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    i.drv_memc_set_ltpo_mode                 0x00016338   Section        0  drv_memc.o(i.drv_memc_set_ltpo_mode)
    i.drv_memc_set_tear_mode                 0x00016352   Section        0  drv_memc.o(i.drv_memc_set_tear_mode)
    i.drv_memc_set_tear_waveform             0x00016360   Section        0  drv_memc.o(i.drv_memc_set_tear_waveform)
    i.drv_memc_set_vidc_sync_cnt             0x00016388   Section        0  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    i.drv_param_init_get_ccm                 0x00016398   Section        0  drv_param_init.o(i.drv_param_init_get_ccm)
    i.drv_param_init_get_scld_filter_h       0x000163a0   Section        0  drv_param_init.o(i.drv_param_init_get_scld_filter_h)
    i.drv_param_init_get_scld_filter_v       0x000163b4   Section        0  drv_param_init.o(i.drv_param_init_get_scld_filter_v)
    i.drv_param_init_get_sclu_filter         0x000163c8   Section        0  drv_param_init.o(i.drv_param_init_get_sclu_filter)
    i.drv_param_init_set_ccm                 0x000163d0   Section        0  drv_param_init.o(i.drv_param_init_set_ccm)
    i.drv_param_p2r_filter_init              0x000163e4   Section        0  drv_param_init.o(i.drv_param_p2r_filter_init)
    i.drv_phy_get_para                       0x00016408   Section        0  drv_phy_common.o(i.drv_phy_get_para)
    i.drv_pwm_out_enable                     0x0001645c   Section        0  drv_pwm.o(i.drv_pwm_out_enable)
    i.drv_pwm_out_set_control                0x0001647c   Section        0  drv_pwm.o(i.drv_pwm_out_set_control)
    i.drv_pwm_out_set_period                 0x00016488   Section        0  drv_pwm.o(i.drv_pwm_out_set_period)
    i.drv_pwm_out_set_threshold              0x00016494   Section        0  drv_pwm.o(i.drv_pwm_out_set_threshold)
    i.drv_pwr_set_cp_mode                    0x000164a0   Section        0  drv_pwr.o(i.drv_pwr_set_cp_mode)
    i.drv_pwr_set_pvd_mode                   0x000164c0   Section        0  drv_pwr.o(i.drv_pwr_set_pvd_mode)
    i.drv_pwr_set_system_clk_src             0x000164d8   Section        0  drv_pwr.o(i.drv_pwr_set_system_clk_src)
    i.drv_rx_phy_test_clear                  0x00016508   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_clear)
    drv_rx_phy_test_clear                    0x00016509   Thumb Code    28  drv_dsi_rx.o(i.drv_rx_phy_test_clear)
    i.drv_rx_phy_test_lock                   0x00016524   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_lock)
    drv_rx_phy_test_lock                     0x00016525   Thumb Code    32  drv_dsi_rx.o(i.drv_rx_phy_test_lock)
    i.drv_rx_phy_test_write                  0x00016544   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_write)
    drv_rx_phy_test_write                    0x00016545   Thumb Code    66  drv_dsi_rx.o(i.drv_rx_phy_test_write)
    i.drv_rx_phy_test_write_1_byte           0x00016586   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte)
    drv_rx_phy_test_write_1_byte             0x00016587   Thumb Code    14  drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte)
    i.drv_rx_phy_test_write_2_byte           0x00016594   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte)
    drv_rx_phy_test_write_2_byte             0x00016595   Thumb Code    16  drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte)
    i.drv_rxbr_clear_pkt_buffer              0x000165a4   Section        0  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    i.drv_rxbr_clear_status0                 0x000165ae   Section        0  drv_rxbr.o(i.drv_rxbr_clear_status0)
    i.drv_rxbr_enable_irq                    0x000165b2   Section        0  drv_rxbr.o(i.drv_rxbr_enable_irq)
    i.drv_rxbr_frame_drop_cfg                0x0001660c   Section        0  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    i.drv_rxbr_get_clk                       0x00016620   Section        0  drv_rxbr.o(i.drv_rxbr_get_clk)
    i.drv_rxbr_get_col_addr                  0x0001665c   Section        0  drv_rxbr.o(i.drv_rxbr_get_col_addr)
    i.drv_rxbr_get_int_source                0x00016660   Section        0  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    drv_rxbr_get_int_source                  0x00016661   Thumb Code    18  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    i.drv_rxbr_get_page_addr                 0x00016672   Section        0  drv_rxbr.o(i.drv_rxbr_get_page_addr)
    i.drv_rxbr_get_status0                   0x00016676   Section        0  hal_internal_vsync.o(i.drv_rxbr_get_status0)
    drv_rxbr_get_status0                     0x00016677   Thumb Code    18  hal_internal_vsync.o(i.drv_rxbr_get_status0)
    i.drv_rxbr_hline_rcv0_cfg                0x00016688   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg)
    i.drv_rxbr_hline_rcv_cfg                 0x00016694   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    i.drv_rxbr_register_irq0_callback        0x0001669c   Section        0  drv_rxbr.o(i.drv_rxbr_register_irq0_callback)
    i.drv_rxbr_register_irq1_callback        0x000166a8   Section        0  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    i.drv_rxbr_set_ack_pkt_header            0x000166b4   Section        0  drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header)
    i.drv_rxbr_set_cmd_filter                0x000166c8   Section        0  drv_rxbr.o(i.drv_rxbr_set_cmd_filter)
    i.drv_rxbr_set_color_format              0x00016794   Section        0  drv_rxbr.o(i.drv_rxbr_set_color_format)
    i.drv_rxbr_set_inten                     0x000167a8   Section        0  drv_rxbr.o(i.drv_rxbr_set_inten)
    i.drv_rxbr_set_ltpo_drop_th              0x000167bc   Section        0  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    i.drv_rxbr_set_usr_cfg                   0x000167cc   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    i.drv_rxbr_set_usr_col                   0x000167f2   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    i.drv_rxbr_set_usr_row                   0x000167fa   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    i.drv_spi_m_read_data                    0x00016804   Section        0  drv_spi_master.o(i.drv_spi_m_read_data)
    i.drv_swire_set_int                      0x00016824   Section        0  drv_swire.o(i.drv_swire_set_int)
    i.drv_swire_set_power_down               0x0001686c   Section        0  drv_swire.o(i.drv_swire_set_power_down)
    i.drv_sys_cfg_clear_all_int              0x00016888   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    i.drv_sys_cfg_clear_pending              0x00016894   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    i.drv_sys_cfg_sel_ap_rst_lvl_trig        0x000168bc   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig)
    i.drv_sys_cfg_sel_ap_rst_trig            0x000168d4   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig)
    i.drv_sys_cfg_sel_gpio_group             0x000168f0   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group)
    i.drv_sys_cfg_sel_int_trig               0x00016914   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig)
    i.drv_sys_cfg_set_dma_rx_req             0x00016938   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req)
    i.drv_sys_cfg_set_dma_tx_req             0x00016948   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req)
    i.drv_sys_cfg_set_int                    0x00016958   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    i.drv_timer_clear_status_flags           0x0001697c   Section        0  drv_timer.o(i.drv_timer_clear_status_flags)
    i.drv_timer_enable                       0x00016996   Section        0  drv_timer.o(i.drv_timer_enable)
    i.drv_timer_get_instance                 0x000169b8   Section        0  drv_timer.o(i.drv_timer_get_instance)
    i.drv_timer_get_prescaler                0x000169c4   Section        0  drv_timer.o(i.drv_timer_get_prescaler)
    i.drv_timer_register_callback            0x000169d4   Section        0  drv_timer.o(i.drv_timer_register_callback)
    i.drv_timer_set_current_count            0x000169e4   Section        0  drv_timer.o(i.drv_timer_set_current_count)
    i.drv_timer_set_int                      0x000169f0   Section        0  drv_timer.o(i.drv_timer_set_int)
    i.drv_timer_set_match                    0x00016a38   Section        0  drv_timer.o(i.drv_timer_set_match)
    i.drv_timer_set_prescaler                0x00016a44   Section        0  drv_timer.o(i.drv_timer_set_prescaler)
    i.drv_tx_phy_test_clear                  0x00016a5a   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_clear)
    i.drv_tx_phy_test_enter                  0x00016a66   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    i.drv_tx_phy_test_exit                   0x00016a82   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    i.drv_tx_phy_test_write                  0x00016a9e   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write)
    i.drv_tx_phy_test_write_1_byte           0x00016ab8   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte)
    i.drv_tx_phy_test_write_2_byte           0x00016ac6   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte)
    i.drv_tx_phy_test_write_code             0x00016ad8   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    i.drv_tx_phy_test_write_data             0x00016afa   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_data)
    drv_tx_phy_test_write_data               0x00016afb   Thumb Code    34  drv_dsi_tx.o(i.drv_tx_phy_test_write_data)
    i.drv_vidc_clear_irq                     0x00016b1c   Section        0  drv_vidc.o(i.drv_vidc_clear_irq)
    i.drv_vidc_enable                        0x00016b24   Section        0  drv_vidc.o(i.drv_vidc_enable)
    i.drv_vidc_enable_irq                    0x00016b3c   Section        0  drv_vidc.o(i.drv_vidc_enable_irq)
    i.drv_vidc_get_irq_status                0x00016b7c   Section        0  drv_vidc.o(i.drv_vidc_get_irq_status)
    i.drv_vidc_init_module_enable            0x00016b90   Section        0  drv_vidc.o(i.drv_vidc_init_module_enable)
    i.drv_vidc_register_callback             0x00016bb8   Section        0  drv_vidc.o(i.drv_vidc_register_callback)
    i.drv_vidc_reset                         0x00016bc4   Section        0  drv_vidc.o(i.drv_vidc_reset)
    i.drv_vidc_set_dst_parameter             0x00016bca   Section        0  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    i.drv_vidc_set_irqen                     0x00016c06   Section        0  drv_vidc.o(i.drv_vidc_set_irqen)
    i.drv_vidc_set_mirror                    0x00016c1a   Section        0  drv_vidc.o(i.drv_vidc_set_mirror)
    i.drv_vidc_set_p2r_hcoef0                0x00016c2a   Section        0  drv_vidc.o(i.drv_vidc_set_p2r_hcoef0)
    i.drv_vidc_set_p2r_hinitb                0x00016c32   Section        0  drv_vidc.o(i.drv_vidc_set_p2r_hinitb)
    i.drv_vidc_set_p2r_hinitr                0x00016c58   Section        0  drv_vidc.o(i.drv_vidc_set_p2r_hinitr)
    i.drv_vidc_set_pentile_swap              0x00016c80   Section        0  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    i.drv_vidc_set_pu_ctrl                   0x00016c98   Section        0  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    i.drv_vidc_set_rotation                  0x00016ca2   Section        0  drv_vidc.o(i.drv_vidc_set_rotation)
    i.drv_vidc_set_scld_hcoef0               0x00016cb2   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    i.drv_vidc_set_scld_hcoef1               0x00016cbc   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    i.drv_vidc_set_scld_step                 0x00016cc6   Section        0  drv_vidc.o(i.drv_vidc_set_scld_step)
    i.drv_vidc_set_scld_vcoef0               0x00016cd8   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    i.drv_vidc_set_scld_vcoef1               0x00016ce2   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    i.drv_vidc_set_src_parameter             0x00016cec   Section        0  drv_vidc.o(i.drv_vidc_set_src_parameter)
    i.drv_wdg_clear_edge_flag                0x00016d04   Section        0  drv_wdg.o(i.drv_wdg_clear_edge_flag)
    drv_wdg_clear_edge_flag                  0x00016d05   Thumb Code    12  drv_wdg.o(i.drv_wdg_clear_edge_flag)
    i.drv_wdg_read_edge_flag                 0x00016d14   Section        0  drv_wdg.o(i.drv_wdg_read_edge_flag)
    drv_wdg_read_edge_flag                   0x00016d15   Thumb Code    10  drv_wdg.o(i.drv_wdg_read_edge_flag)
    i.drv_wdg_set_int                        0x00016d24   Section        0  drv_wdg.o(i.drv_wdg_set_int)
    i.fls_clr_interrupt_flag                 0x00016d58   Section        0  drv_fls.o(i.fls_clr_interrupt_flag)
    i.fputc                                  0x00016d62   Section        0  tau_log.o(i.fputc)
    i.hal_dsi_rx_ctrl_create_handle          0x00016d78   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    i.hal_dsi_rx_ctrl_deinit                 0x00016da8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit)
    i.hal_dsi_rx_ctrl_dsc_async_handler      0x00016dcc   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler)
    i.hal_dsi_rx_ctrl_gen_a_tear_signal      0x00016e50   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal)
    i.hal_dsi_rx_ctrl_get_max_ret_size       0x00016e78   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size)
    i.hal_dsi_rx_ctrl_init                   0x00016ea0   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    i.hal_dsi_rx_ctrl_init_clk               0x00016f38   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    hal_dsi_rx_ctrl_init_clk                 0x00016f39   Thumb Code   554  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    i.hal_dsi_rx_ctrl_init_dsi_rx            0x00017200   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    hal_dsi_rx_ctrl_init_dsi_rx              0x00017201   Thumb Code   182  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    i.hal_dsi_rx_ctrl_init_memc              0x000172c8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    hal_dsi_rx_ctrl_init_memc                0x000172c9   Thumb Code   308  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    i.hal_dsi_rx_ctrl_init_rxbr              0x00017404   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    hal_dsi_rx_ctrl_init_rxbr                0x00017405   Thumb Code   266  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    i.hal_dsi_rx_ctrl_init_vidc              0x00017520   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    hal_dsi_rx_ctrl_init_vidc                0x00017521   Thumb Code   544  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    i.hal_dsi_rx_ctrl_pre_init_pps           0x0001774c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    i.hal_dsi_rx_ctrl_send_ack_cmd           0x00017788   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd)
    i.hal_dsi_rx_ctrl_set_cus_esc_clk        0x00017878   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk)
    i.hal_dsi_rx_ctrl_set_cus_sync_line      0x000178a4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line)
    i.hal_dsi_rx_ctrl_set_hw_tear_mode       0x000178d8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode)
    i.hal_dsi_rx_ctrl_set_sw_tear_mode       0x0001790c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode)
    i.hal_dsi_rx_ctrl_start                  0x00017940   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    i.hal_dsi_rx_ctrl_stop                   0x0001797c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop)
    i.hal_dsi_rx_ctrl_toggle_resolution      0x000179b8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    i.hal_dsi_tx_calc_video_chunks           0x000179d8   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks)
    hal_dsi_tx_calc_video_chunks             0x000179d9   Thumb Code   384  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks)
    i.hal_dsi_tx_count_lane_rate             0x00017b68   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate)
    hal_dsi_tx_count_lane_rate               0x00017b69   Thumb Code  1286  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate)
    i.hal_dsi_tx_ctrl_create_handle          0x00018074   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    i.hal_dsi_tx_ctrl_deinit                 0x000180a0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit)
    i.hal_dsi_tx_ctrl_enter_init_panel_mode  0x000180e8   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode)
    i.hal_dsi_tx_ctrl_exit_init_panel_mode   0x00018134   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode)
    i.hal_dsi_tx_ctrl_init                   0x0001815c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    i.hal_dsi_tx_ctrl_init_clk               0x00018200   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    hal_dsi_tx_ctrl_init_clk                 0x00018201   Thumb Code    36  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    i.hal_dsi_tx_ctrl_panel_reset_pin        0x00018224   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin)
    i.hal_dsi_tx_ctrl_set_ccm                0x00018230   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm)
    i.hal_dsi_tx_ctrl_set_overwrite_rgb      0x00018250   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    i.hal_dsi_tx_ctrl_set_partial_disp       0x00018264   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp)
    i.hal_dsi_tx_ctrl_set_partial_disp_area  0x00018274   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area)
    i.hal_dsi_tx_ctrl_start                  0x00018298   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    i.hal_dsi_tx_ctrl_stop                   0x00018304   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop)
    i.hal_dsi_tx_ctrl_write_array_cmd        0x00018348   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd)
    i.hal_dsi_tx_ctrl_write_cmd              0x00018420   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    i.hal_dsi_tx_init_data_mode              0x000184d0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode)
    hal_dsi_tx_init_data_mode                0x000184d1   Thumb Code    58  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode)
    i.hal_dsi_tx_init_dpi_cfg                0x00018514   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg)
    hal_dsi_tx_init_dpi_cfg                  0x00018515   Thumb Code    42  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg)
    i.hal_dsi_tx_init_interrupt              0x00018544   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt)
    hal_dsi_tx_init_interrupt                0x00018545   Thumb Code    28  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt)
    i.hal_dsi_tx_init_phy_cfg                0x00018564   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    hal_dsi_tx_init_phy_cfg                  0x00018565   Thumb Code    28  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    i.hal_dsi_tx_init_remains                0x00018584   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains)
    hal_dsi_tx_init_remains                  0x00018585   Thumb Code   142  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains)
    i.hal_dsi_tx_init_video_mode             0x00018618   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode)
    hal_dsi_tx_init_video_mode               0x00018619   Thumb Code    82  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode)
    i.hal_dsi_tx_phy_test_get_data           0x00018670   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_phy_test_get_data)
    hal_dsi_tx_phy_test_get_data             0x00018671   Thumb Code   108  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_phy_test_get_data)
    i.hal_dsi_tx_phy_test_setup              0x000186e0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_phy_test_setup)
    hal_dsi_tx_phy_test_setup                0x000186e1   Thumb Code   244  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_phy_test_setup)
    i.hal_dsi_tx_send_cmd                    0x000187d4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    hal_dsi_tx_send_cmd                      0x000187d5   Thumb Code    60  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    i.hal_gpio_ctrl_eint                     0x00018818   Section        0  hal_gpio.o(i.hal_gpio_ctrl_eint)
    i.hal_gpio_get_input_data                0x00018830   Section        0  hal_gpio.o(i.hal_gpio_get_input_data)
    i.hal_gpio_init_eint                     0x00018844   Section        0  hal_gpio.o(i.hal_gpio_init_eint)
    i.hal_gpio_init_output                   0x00018884   Section        0  hal_gpio.o(i.hal_gpio_init_output)
    i.hal_gpio_reg_eint_cb                   0x000188ac   Section        0  hal_gpio.o(i.hal_gpio_reg_eint_cb)
    i.hal_gpio_set_ap_reset_int              0x000188c4   Section        0  hal_gpio.o(i.hal_gpio_set_ap_reset_int)
    i.hal_gpio_set_mode                      0x00018914   Section        0  hal_gpio.o(i.hal_gpio_set_mode)
    i.hal_gpio_set_output_data               0x00018974   Section        0  hal_gpio.o(i.hal_gpio_set_output_data)
    i.hal_gpio_set_pull_state                0x0001897c   Section        0  hal_gpio.o(i.hal_gpio_set_pull_state)
    i.hal_i2c_m_dma_init                     0x0001899c   Section        0  hal_i2c_master.o(i.hal_i2c_m_dma_init)
    i.hal_i2c_m_dma_read                     0x00018a08   Section        0  hal_i2c_master.o(i.hal_i2c_m_dma_read)
    i.hal_i2c_m_dma_write                    0x00018a28   Section        0  hal_i2c_master.o(i.hal_i2c_m_dma_write)
    i.hal_i2c_m_transfer_complate            0x00018a44   Section        0  hal_i2c_master.o(i.hal_i2c_m_transfer_complate)
    i.hal_i2c_master_irq_callback            0x00018a50   Section        0  hal_i2c_master.o(i.hal_i2c_master_irq_callback)
    hal_i2c_master_irq_callback              0x00018a51   Thumb Code    24  hal_i2c_master.o(i.hal_i2c_master_irq_callback)
    i.hal_i2c_s_dma_user_callback            0x00018a70   Section        0  hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback)
    hal_i2c_s_dma_user_callback              0x00018a71   Thumb Code    12  hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback)
    i.hal_i2c_s_dma_write                    0x00018a80   Section        0  hal_i2c_slave.o(i.hal_i2c_s_dma_write)
    i.hal_i2c_s_init                         0x00018ab8   Section        0  hal_i2c_slave.o(i.hal_i2c_s_init)
    i.hal_i2c_s_nonblocking_read             0x00018b24   Section        0  hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read)
    i.hal_i2c_s_set_transfer                 0x00018b38   Section        0  hal_i2c_slave.o(i.hal_i2c_s_set_transfer)
    i.hal_i2c_slave_irq_callback             0x00018b44   Section        0  hal_i2c_slave.o(i.hal_i2c_slave_irq_callback)
    hal_i2c_slave_irq_callback               0x00018b45   Thumb Code   258  hal_i2c_slave.o(i.hal_i2c_slave_irq_callback)
    i.hal_internal_init_memc                 0x00018c5c   Section        0  hal_internal_vsync.o(i.hal_internal_init_memc)
    i.hal_internal_sync_get_fb_setting       0x00018d40   Section        0  hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting)
    i.hal_internal_sync_input_resolution_change 0x00018d50   Section        0  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    i.hal_internal_vsync_deinit              0x00018f64   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    i.hal_internal_vsync_get_sync_line       0x00018f80   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    i.hal_internal_vsync_init_rx             0x00018f98   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    i.hal_internal_vsync_init_tx             0x00019094   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    i.hal_internal_vsync_set_auto_hw_filter  0x00019144   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter)
    i.hal_internal_vsync_set_rx_state        0x00019260   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    i.hal_internal_vsync_set_sync_line       0x00019274   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line)
    i.hal_internal_vsync_set_tear_mode       0x00019290   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    i.hal_internal_vsync_set_tx_state        0x000192d4   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    i.hal_lcdc_config_ccm                    0x00019314   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm)
    hal_lcdc_config_ccm                      0x00019315   Thumb Code    30  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm)
    i.hal_lcdc_config_remains                0x00019338   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains)
    hal_lcdc_config_remains                  0x00019339   Thumb Code    68  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains)
    i.hal_lcdc_config_rgb_to_pentile         0x00019380   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile)
    hal_lcdc_config_rgb_to_pentile           0x00019381   Thumb Code    14  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile)
    i.hal_lcdc_config_upscaler               0x00019394   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler)
    hal_lcdc_config_upscaler                 0x00019395   Thumb Code   346  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler)
    i.hal_lcdc_init_cfg                      0x000194f8   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    hal_lcdc_init_cfg                        0x000194f9   Thumb Code    60  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    i.hal_lcdc_init_clk                      0x00019538   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    hal_lcdc_init_clk                        0x00019539   Thumb Code   288  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    i.hal_lcdc_init_interrupt                0x0001966c   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt)
    hal_lcdc_init_interrupt                  0x0001966d   Thumb Code    58  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt)
    i.hal_pwm_out_config_all                 0x000196ac   Section        0  hal_pwm.o(i.hal_pwm_out_config_all)
    i.hal_pwm_out_init                       0x00019714   Section        0  hal_pwm.o(i.hal_pwm_out_init)
    i.hal_spi_m_clear_rxfifo                 0x00019720   Section        0  hal_spi_master.o(i.hal_spi_m_clear_rxfifo)
    i.hal_swire_open                         0x0001972e   Section        0  hal_swire.o(i.hal_swire_open)
    i.hal_system_enable_systick              0x00019744   Section        0  hal_system.o(i.hal_system_enable_systick)
    i.hal_system_init                        0x0001974c   Section        0  hal_system.o(i.hal_system_init)
    i.hal_system_init_console                0x000197c8   Section        0  hal_system.o(i.hal_system_init_console)
    i.hal_system_set_pvd                     0x000197e4   Section        0  hal_system.o(i.hal_system_set_pvd)
    i.hal_system_set_vcc                     0x000197ec   Section        0  hal_system.o(i.hal_system_set_vcc)
    i.hal_timer_init                         0x000197f4   Section        0  hal_timer.o(i.hal_timer_init)
    i.hal_timer_start                        0x00019818   Section        0  hal_timer.o(i.hal_timer_start)
    i.hal_timer_stop                         0x0001986c   Section        0  hal_timer.o(i.hal_timer_stop)
    i.hal_uart_init                          0x00019894   Section        0  hal_uart.o(i.hal_uart_init)
    i.hal_uart_transmit_blocking             0x00019920   Section        0  hal_uart.o(i.hal_uart_transmit_blocking)
    i.handle_init                            0x00019930   Section        0  irq_redirect .o(i.handle_init)
    i.init_mipi_tx                           0x00019a40   Section        0  ap_demo.o(i.init_mipi_tx)
    init_mipi_tx                             0x00019a41   Thumb Code   102  ap_demo.o(i.init_mipi_tx)
    i.init_panel                             0x00019ab0   Section        0  ap_demo.o(i.init_panel)
    init_panel                               0x00019ab1   Thumb Code   194  ap_demo.o(i.init_panel)
    i.main                                   0x00019bac   Section        0  main.o(i.main)
    i.open_mipi_rx                           0x00019bb8   Section        0  ap_demo.o(i.open_mipi_rx)
    open_mipi_rx                             0x00019bb9   Thumb Code   144  ap_demo.o(i.open_mipi_rx)
    i.pps_update_handle                      0x00019c68   Section        0  ap_demo.o(i.pps_update_handle)
    pps_update_handle                        0x00019c69   Thumb Code    62  ap_demo.o(i.pps_update_handle)
    i.rx_get_dcs_packet_data                 0x00019cd4   Section        0  hal_internal_vsync.o(i.rx_get_dcs_packet_data)
    rx_get_dcs_packet_data                   0x00019cd5   Thumb Code   654  hal_internal_vsync.o(i.rx_get_dcs_packet_data)
    i.rx_partial_update                      0x0001a0c8   Section        0  hal_internal_vsync.o(i.rx_partial_update)
    rx_partial_update                        0x0001a0c9   Thumb Code   304  hal_internal_vsync.o(i.rx_partial_update)
    i.rx_receive_packet                      0x0001a208   Section        0  hal_internal_vsync.o(i.rx_receive_packet)
    rx_receive_packet                        0x0001a209   Thumb Code   128  hal_internal_vsync.o(i.rx_receive_packet)
    i.rx_receive_pps                         0x0001a294   Section        0  hal_internal_vsync.o(i.rx_receive_pps)
    rx_receive_pps                           0x0001a295   Thumb Code   268  hal_internal_vsync.o(i.rx_receive_pps)
    i.rxbr_irq0_callback                     0x0001a414   Section        0  hal_internal_vsync.o(i.rxbr_irq0_callback)
    rxbr_irq0_callback                       0x0001a415   Thumb Code   158  hal_internal_vsync.o(i.rxbr_irq0_callback)
    i.rxbr_irq1_callback                     0x0001a4b8   Section        0  hal_internal_vsync.o(i.rxbr_irq1_callback)
    rxbr_irq1_callback                       0x0001a4b9   Thumb Code   222  hal_internal_vsync.o(i.rxbr_irq1_callback)
    i.soft_gen_te                            0x0001a628   Section        0  hal_internal_vsync.o(i.soft_gen_te)
    soft_gen_te                              0x0001a629   Thumb Code   116  hal_internal_vsync.o(i.soft_gen_te)
    i.soft_timer3_cb                         0x0001a6b4   Section        0  ap_demo.o(i.soft_timer3_cb)
    soft_timer3_cb                           0x0001a6b5   Thumb Code    36  ap_demo.o(i.soft_timer3_cb)
    i.vidc_callback                          0x0001a6e4   Section        0  hal_internal_vsync.o(i.vidc_callback)
    vidc_callback                            0x0001a6e5   Thumb Code   146  hal_internal_vsync.o(i.vidc_callback)
    i.vpre_err_reset                         0x0001a798   Section        0  hal_internal_vsync.o(i.vpre_err_reset)
    vpre_err_reset                           0x0001a799   Thumb Code   184  hal_internal_vsync.o(i.vpre_err_reset)
    i.vsync_set_te_mode                      0x0001a868   Section        0  hal_internal_vsync.o(i.vsync_set_te_mode)
    vsync_set_te_mode                        0x0001a869   Thumb Code   254  hal_internal_vsync.o(i.vsync_set_te_mode)
    .constdata                               0x0001aa04   Section    13212  ap_demo.o(.constdata)
    g_cus_rx_dcs_execute_table               0x0001aa04   Data         108  ap_demo.o(.constdata)
    .constdata                               0x0001dda0   Section     2354  app_tp_for_custom_s8.o(.constdata)
    .constdata                               0x0001e6d2   Section        1  app_tp_for_custom_s8.o(.constdata)
    .constdata                               0x0001e6d4   Section      260  hal_dsi_tx_ctrl.o(.constdata)
    data_high_map                            0x0001e6d4   Data         160  hal_dsi_tx_ctrl.o(.constdata)
    data_lp_map                              0x0001e774   Data         100  hal_dsi_tx_ctrl.o(.constdata)
    .constdata                               0x0001e7d8   Section      210  hal_gpio.o(.constdata)
    s_gpio_map                               0x0001e7d8   Data         120  hal_gpio.o(.constdata)
    s_gpio_perf                              0x0001e850   Data          90  hal_gpio.o(.constdata)
    .constdata                               0x0001e8ac   Section        8  drv_param_init.o(.constdata)
    .constdata                               0x0001e8b4   Section       32  drv_timer.o(.constdata)
    s_timer_map                              0x0001e8b4   Data          32  drv_timer.o(.constdata)
    .constdata                               0x0001e8d4   Section      312  drv_phy_common.o(.constdata)
    phy_para_mapping_h                       0x0001e8d4   Data         184  drv_phy_common.o(.constdata)
    phy_para_mapping_l                       0x0001e98c   Data         128  drv_phy_common.o(.constdata)
    .conststring                             0x0001ea0c   Section       72  hal_dsi_rx_ctrl.o(.conststring)
    .conststring                             0x0001ea54   Section      308  hal_internal_vsync.o(.conststring)
    .ARM.__AT_0x00070100                     0x00070100   Section      192  irq_redirect .o(.ARM.__AT_0x00070100)
    .data                                    0x000701d0   Section       48  ap_demo.o(.data)
    g_calibration_flag                       0x000701d0   Data           1  ap_demo.o(.data)
    start_display_on                         0x000701d1   Data           1  ap_demo.o(.data)
    g_need_enter_sleep_mode                  0x000701d2   Data           1  ap_demo.o(.data)
    g_exit_sleep_mode                        0x000701d3   Data           1  ap_demo.o(.data)
    panel_display_done                       0x000701d4   Data           1  ap_demo.o(.data)
    b3_read_flag                             0x000701d8   Data           1  ap_demo.o(.data)
    c8_read_flag                             0x000701d9   Data           1  ap_demo.o(.data)
    c9_read_flag                             0x000701da   Data           1  ap_demo.o(.data)
    c9_read_flag2                            0x000701db   Data           1  ap_demo.o(.data)
    c9_read_flag3                            0x000701dc   Data           1  ap_demo.o(.data)
    flag_5a                                  0x000701dd   Data           1  ap_demo.o(.data)
    read_bl_data                             0x000701e0   Data           2  ap_demo.o(.data)
    read_bl_data_bak                         0x000701e2   Data           2  ap_demo.o(.data)
    g_rx_ctrl_handle                         0x000701f0   Data           4  ap_demo.o(.data)
    g_tx_ctrl_handle                         0x000701f4   Data           4  ap_demo.o(.data)
    value_reg_df                             0x000701f8   Data           4  ap_demo.o(.data)
    s20_power_on_flag                        0x000701fc   Data           4  ap_demo.o(.data)
    .data                                    0x00070200   Section      228  app_tp_for_custom_s8.o(.data)
    app_tp_count                             0x0007020a   Data           1  app_tp_for_custom_s8.o(.data)
    phone_85_flag                            0x0007020b   Data           1  app_tp_for_custom_s8.o(.data)
    phone_F6_flag                            0x0007020c   Data           1  app_tp_for_custom_s8.o(.data)
    phone_E4_flag                            0x0007020d   Data           1  app_tp_for_custom_s8.o(.data)
    phone_72_flag                            0x0007020e   Data           1  app_tp_for_custom_s8.o(.data)
    phone_75_flag                            0x0007020f   Data           1  app_tp_for_custom_s8.o(.data)
    phone_92_flag                            0x00070210   Data           1  app_tp_for_custom_s8.o(.data)
    phone_74_flag                            0x00070211   Data           1  app_tp_for_custom_s8.o(.data)
    u16CoordY                                0x00070214   Data           2  app_tp_for_custom_s8.o(.data)
    u16CoordX                                0x00070216   Data           2  app_tp_for_custom_s8.o(.data)
    u16CoordY_back                           0x00070218   Data           2  app_tp_for_custom_s8.o(.data)
    u16CoordX_back                           0x0007021a   Data           2  app_tp_for_custom_s8.o(.data)
    .data                                    0x000702e4   Section        1  app_tp_for_custom_s8.o(.data)
    .data                                    0x000702e5   Section        1  app_tp_for_custom_s8.o(.data)
    .data                                    0x000702e6   Section        1  app_tp_for_custom_s8.o(.data)
    .data                                    0x000702e7   Section        3  app_tp_for_custom_s8.o(.data)
    .data                                    0x000702ea   Section        5  app_tp_for_custom_s8.o(.data)
    .data                                    0x000702f0   Section       48  app_tp_for_custom_s8.o(.data)
    .data                                    0x00070320   Section       48  app_tp_transfer.o(.data)
    s_spim_write                             0x00070320   Data           1  app_tp_transfer.o(.data)
    s_screen_int_flag                        0x00070321   Data           1  app_tp_transfer.o(.data)
    s_phone_reset_flag                       0x00070322   Data           1  app_tp_transfer.o(.data)
    s_screen_int_transfer_status             0x00070323   Data           1  app_tp_transfer.o(.data)
    s_screen_const_transfer_count            0x00070325   Data           1  app_tp_transfer.o(.data)
    screen_int_transfer_count                0x00070326   Data           1  app_tp_transfer.o(.data)
    screen_int_transfer_buffer_ready         0x00070327   Data           1  app_tp_transfer.o(.data)
    .data                                    0x00070350   Section        8  hal_dsi_rx_ctrl.o(.data)
    g_hw_auto_filter                         0x00070350   Data           1  hal_dsi_rx_ctrl.o(.data)
    g_esc_clk                                0x00070354   Data           4  hal_dsi_rx_ctrl.o(.data)
    .data                                    0x00070358   Section        1  hal_dsi_tx_ctrl.o(.data)
    g_tx_mode                                0x00070358   Data           1  hal_dsi_tx_ctrl.o(.data)
    .data                                    0x00070359   Section        1  hal_i2c_master.o(.data)
    s_i2c_m_transfer_end                     0x00070359   Data           1  hal_i2c_master.o(.data)
    .data                                    0x0007035c   Section       28  hal_i2c_slave.o(.data)
    s_txbuffer_complate                      0x0007035c   Data           1  hal_i2c_slave.o(.data)
    s_i2c_s_dma_end                          0x0007035d   Data           1  hal_i2c_slave.o(.data)
    s_i2c_s_receive_cnt                      0x0007035e   Data           1  hal_i2c_slave.o(.data)
    s_hal_slave_rxbuffer                     0x00070360   Data           4  hal_i2c_slave.o(.data)
    s_hal_slave_rxbuffer_size                0x00070364   Data           4  hal_i2c_slave.o(.data)
    hal_i2c_s_callback                       0x00070368   Data           4  hal_i2c_slave.o(.data)
    s_receive_count                          0x0007036c   Data           4  hal_i2c_slave.o(.data)
    s_tx_buffer_t                            0x00070370   Data           4  hal_i2c_slave.o(.data)
    tx_sum                                   0x00070374   Data           4  hal_i2c_slave.o(.data)
    .data                                    0x00070378   Section        4  hal_internal_vsync.o(.data)
    sg_cur_te_info                           0x00070378   Data           4  hal_internal_vsync.o(.data)
    .data                                    0x0007037c   Section       18  norflash.o(.data)
    tmprg                                    0x00070384   Data           4  norflash.o(.data)
    .data                                    0x00070390   Section       12  drv_common.o(.data)
    s_my_tick                                0x00070390   Data           4  drv_common.o(.data)
    .data                                    0x0007039c   Section        4  drv_gpio.o(.data)
    g_ap_reset_cb                            0x0007039c   Data           4  drv_gpio.o(.data)
    .data                                    0x000703a0   Section        8  drv_i2c_dma.o(.data)
    i2c0_dma_callback                        0x000703a0   Data           4  drv_i2c_dma.o(.data)
    i2c1_dma_callback                        0x000703a4   Data           4  drv_i2c_dma.o(.data)
    .data                                    0x000703a8   Section     1188  drv_param_init.o(.data)
    .data                                    0x0007084c   Section       12  drv_pwm.o(.data)
    s_pwm_type                               0x0007084c   Data           1  drv_pwm.o(.data)
    s_pwm_cb                                 0x00070850   Data           8  drv_pwm.o(.data)
    .data                                    0x00070858   Section        8  drv_rxbr.o(.data)
    .data                                    0x00070860   Section        8  drv_swire.o(.data)
    s_swire_cb                               0x00070860   Data           8  drv_swire.o(.data)
    .data                                    0x00070868   Section        1  drv_sys_cfg.o(.data)
    sg_ap_rstn_trigger_type                  0x00070868   Data           1  drv_sys_cfg.o(.data)
    .data                                    0x0007086c   Section        4  drv_vidc.o(.data)
    .data                                    0x00070870   Section        4  drv_i2c_master.o(.data)
    i2c1_intr_callback                       0x00070870   Data           4  drv_i2c_master.o(.data)
    .data                                    0x00070874   Section        8  drv_i2c_slave.o(.data)
    i2c0_intr_callback                       0x00070874   Data           4  drv_i2c_slave.o(.data)
    .data                                    0x0007087c   Section        4  drv_spi_master.o(.data)
    SPIM_intr_callback                       0x0007087c   Data           4  drv_spi_master.o(.data)
    .data                                    0x00070880   Section       12  drv_chip_info.o(.data)
    sg_chip_info                             0x00070880   Data           4  drv_chip_info.o(.data)
    sg_chip_function                         0x00070884   Data           4  drv_chip_info.o(.data)
    sg_chip_encrypt                          0x00070888   Data           4  drv_chip_info.o(.data)
    .data                                    0x0007088c   Section        8  drv_uart.o(.data)
    s_UartFcrReg                             0x0007088c   Data           4  drv_uart.o(.data)
    uart_userData                            0x00070890   Data           4  drv_uart.o(.data)
    .data                                    0x00070894   Section        8  drv_wdg.o(.data)
    s_wdg_cb                                 0x00070894   Data           8  drv_wdg.o(.data)
    .data                                    0x0007089c   Section        4  stdout.o(.data)
    .bss                                     0x000708a0   Section      400  app_tp_transfer.o(.bss)
    s_screen_read_buffer                     0x000708a0   Data         200  app_tp_transfer.o(.bss)
    s_phone_read_buffer                      0x00070968   Data         200  app_tp_transfer.o(.bss)
    .bss                                     0x00070a30   Section      192  hal_dsi_rx_ctrl.o(.bss)
    g_rx_ctrl_handle                         0x00070a30   Data         192  hal_dsi_rx_ctrl.o(.bss)
    .bss                                     0x00070af0   Section       72  hal_dsi_tx_ctrl.o(.bss)
    g_tx_ctrl_handle                         0x00070af0   Data          72  hal_dsi_tx_ctrl.o(.bss)
    .bss                                     0x00070b38   Section      256  tau_log.o(.bss)
    .bss                                     0x00070c38   Section      208  hal_uart.o(.bss)
    .bss                                     0x00070d08   Section     2392  hal_internal_vsync.o(.bss)
    g_imm_buffer                             0x00071540   Data         255  hal_internal_vsync.o(.bss)
    sg_te_info                               0x00071640   Data          12  hal_internal_vsync.o(.bss)
    g_imm_packet                             0x0007164c   Data          20  hal_internal_vsync.o(.bss)
    .bss                                     0x00071660   Section     4144  dcs_packet_fifo.o(.bss)
    .bss                                     0x00072690   Section       28  drv_dma.o(.bss)
    s_dma_handle                             0x00072690   Data          28  drv_dma.o(.bss)
    .bss                                     0x000726ac   Section       64  drv_gpio.o(.bss)
    s_gpio_cb                                0x000726ac   Data          64  drv_gpio.o(.bss)
    .bss                                     0x000726ec   Section      320  drv_i2c_dma.o(.bss)
    i2c0_dma_slave_handle                    0x000726ec   Data         160  drv_i2c_dma.o(.bss)
    i2c1_dma_master_handle                   0x0007278c   Data         160  drv_i2c_dma.o(.bss)
    .bss                                     0x0007282c   Section       32  drv_timer.o(.bss)
    s_timer_cb                               0x0007282c   Data          32  drv_timer.o(.bss)
    .bss                                     0x0007284c   Section       32  hal_spi_slave.o(.bss)
    STACK                                    0x00072870   Section     4096  startup_armcm0.o(STACK)

    Global Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    BuildAttributes$$THM_ISAv3M$S$PE$A:L22$X:L11$S22$IEEE1$IW$USESV6$~STKCKD$USESV7$~SHL$OTIME$ROPI$IEEEJ$EBA8$MICROLIB$REQ8$PRES8$EABIv2 0x00000000   Number         0  anon$$obj.o ABSOLUTE
    __ARM_use_no_argv                        0x00000000   Number         0  main.o ABSOLUTE
    _printf_a                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_c                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_charcount                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_d                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_e                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_f                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_flags                            0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_dec                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_hex                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_g                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_i                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_int_dec                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_l                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ll                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lld                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lli                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llo                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llu                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llx                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_dec                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_hex                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_oct                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ls                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_mbtowc                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_n                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_o                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_p                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_percent                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_pre_padding                      0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_return_value                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_s                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_sizespec                         0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_str                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_signed                  0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_unsigned                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_u                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wctomb                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_widthprec                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_x                                0x00000000   Number         0  stubs.o ABSOLUTE
    __cpp_initialize__aeabi_                  - Undefined Weak Reference
    __cxa_finalize                            - Undefined Weak Reference
    _clock_init                               - Undefined Weak Reference
    _microlib_exit                            - Undefined Weak Reference
    __Vectors_Size                           0x000000c0   Number         0  startup_armcm0.o ABSOLUTE
    __Vectors                                0x00010000   Data           4  startup_armcm0.o(RESET)
    __Vectors_End                            0x000100c0   Data           0  startup_armcm0.o(RESET)
    __main                                   0x000100c1   Thumb Code     0  entry.o(.ARM.Collect$$$$00000000)
    _main_stk                                0x000100c1   Thumb Code     0  entry2.o(.ARM.Collect$$$$00000001)
    _main_scatterload                        0x000100c5   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    __main_after_scatterload                 0x000100c9   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    _main_clock                              0x000100c9   Thumb Code     0  entry7b.o(.ARM.Collect$$$$00000008)
    _main_cpp_init                           0x000100c9   Thumb Code     0  entry8b.o(.ARM.Collect$$$$0000000A)
    _main_init                               0x000100c9   Thumb Code     0  entry9a.o(.ARM.Collect$$$$0000000B)
    __rt_final_cpp                           0x000100d1   Thumb Code     0  entry10a.o(.ARM.Collect$$$$0000000D)
    __rt_final_exit                          0x000100d1   Thumb Code     0  entry11a.o(.ARM.Collect$$$$0000000F)
    Reset_Handler                            0x000100d5   Thumb Code    28  startup_armcm0.o(.text)
    NMI_Handler                              0x000100f1   Thumb Code     2  startup_armcm0.o(.text)
    SVC_Handler                              0x000100f5   Thumb Code     2  startup_armcm0.o(.text)
    PendSV_Handler                           0x000100f7   Thumb Code     2  startup_armcm0.o(.text)
    OTP_IRQn_Handler                         0x00010123   Thumb Code     2  startup_armcm0.o(.text)
    PVD_IRQn_Handler                         0x00010127   Thumb Code     2  startup_armcm0.o(.text)
    __aeabi_uidiv                            0x0001014d   Thumb Code     0  uidiv.o(.text)
    __aeabi_uidivmod                         0x0001014d   Thumb Code    44  uidiv.o(.text)
    __aeabi_idiv                             0x00010179   Thumb Code     0  idiv.o(.text)
    __aeabi_idivmod                          0x00010179   Thumb Code    40  idiv.o(.text)
    __aeabi_memcpy                           0x000101a1   Thumb Code    36  memcpya.o(.text)
    __aeabi_memcpy4                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memcpy8                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memset                           0x000101c5   Thumb Code    14  memseta.o(.text)
    __aeabi_memset4                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memset8                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr                           0x000101d3   Thumb Code     4  memseta.o(.text)
    __aeabi_memclr4                          0x000101d3   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr8                          0x000101d3   Thumb Code     0  memseta.o(.text)
    _memset$wrapper                          0x000101d7   Thumb Code    18  memseta.o(.text)
    __aeabi_fadd                             0x000101e9   Thumb Code   162  fadd.o(.text)
    __aeabi_fsub                             0x0001028b   Thumb Code     8  fadd.o(.text)
    __aeabi_frsub                            0x00010293   Thumb Code     8  fadd.o(.text)
    __aeabi_fmul                             0x0001029b   Thumb Code   122  fmul.o(.text)
    __aeabi_fdiv                             0x00010315   Thumb Code   124  fdiv.o(.text)
    __ARM_scalbnf                            0x00010391   Thumb Code    24  fscalb.o(.text)
    scalbnf                                  0x00010391   Thumb Code     0  fscalb.o(.text)
    __aeabi_dadd                             0x000103a9   Thumb Code   328  dadd.o(.text)
    __aeabi_dsub                             0x000104f1   Thumb Code    12  dadd.o(.text)
    __aeabi_drsub                            0x000104fd   Thumb Code    12  dadd.o(.text)
    __aeabi_dmul                             0x0001050d   Thumb Code   202  dmul.o(.text)
    __aeabi_ddiv                             0x000105dd   Thumb Code   234  ddiv.o(.text)
    __aeabi_i2f                              0x000106cd   Thumb Code    22  fflti.o(.text)
    __aeabi_ui2f                             0x000106e3   Thumb Code    14  ffltui.o(.text)
    __aeabi_ui2d                             0x000106f1   Thumb Code    24  dfltui.o(.text)
    __aeabi_f2iz                             0x0001070d   Thumb Code    50  ffixi.o(.text)
    __aeabi_f2uiz                            0x0001073f   Thumb Code    40  ffixui.o(.text)
    __aeabi_d2iz                             0x00010769   Thumb Code    62  dfixi.o(.text)
    __aeabi_d2uiz                            0x000107b1   Thumb Code    50  dfixui.o(.text)
    __aeabi_f2d                              0x000107ed   Thumb Code    40  f2d.o(.text)
    __aeabi_cfrcmple                         0x00010815   Thumb Code    20  cfrcmple.o(.text)
    __aeabi_uldivmod                         0x00010829   Thumb Code    96  uldiv.o(.text)
    __aeabi_llsl                             0x00010889   Thumb Code    32  llshl.o(.text)
    _ll_shift_l                              0x00010889   Thumb Code     0  llshl.o(.text)
    __aeabi_llsr                             0x000108a9   Thumb Code    34  llushr.o(.text)
    _ll_ushift_r                             0x000108a9   Thumb Code     0  llushr.o(.text)
    __aeabi_lasr                             0x000108cb   Thumb Code    38  llsshr.o(.text)
    _ll_sshift_r                             0x000108cb   Thumb Code     0  llsshr.o(.text)
    __I$use$fp                               0x000108f1   Thumb Code     0  iusefp.o(.text)
    _float_round                             0x000108f1   Thumb Code    16  fepilogue.o(.text)
    _float_epilogue                          0x00010901   Thumb Code   114  fepilogue.o(.text)
    _double_round                            0x00010973   Thumb Code    26  depilogue.o(.text)
    _double_epilogue                         0x0001098d   Thumb Code   164  depilogue.o(.text)
    __aeabi_d2ulz                            0x00010a31   Thumb Code    54  dfixul.o(.text)
    __aeabi_cdrcmple                         0x00010a71   Thumb Code    38  cdrcmple.o(.text)
    __scatterload                            0x00010a99   Thumb Code    28  init.o(.text)
    __scatterload_rt2                        0x00010a99   Thumb Code     0  init.o(.text)
    __decompress                             0x00010abd   Thumb Code     0  __dczerorl2.o(.text)
    __decompress1                            0x00010abd   Thumb Code    86  __dczerorl2.o(.text)
    ADC_IRQn_Handler                         0x00010b15   Thumb Code    18  irq_redirect .o(i.ADC_IRQn_Handler)
    AP_NRESET_IRQn_Handler                   0x00010b2d   Thumb Code    18  irq_redirect .o(i.AP_NRESET_IRQn_Handler)
    DMA_IRQn_Handler                         0x00010b45   Thumb Code    14  irq_redirect .o(i.DMA_IRQn_Handler)
    EXTI_INT0_IRQn_Handler                   0x00010b59   Thumb Code    22  irq_redirect .o(i.EXTI_INT0_IRQn_Handler)
    EXTI_INT1_IRQn_Handler                   0x00010b75   Thumb Code    22  irq_redirect .o(i.EXTI_INT1_IRQn_Handler)
    EXTI_INT2_IRQn_Handler                   0x00010b91   Thumb Code    22  irq_redirect .o(i.EXTI_INT2_IRQn_Handler)
    EXTI_INT3_IRQn_Handler                   0x00010bad   Thumb Code    22  irq_redirect .o(i.EXTI_INT3_IRQn_Handler)
    EXTI_INT4_IRQn_Handler                   0x00010bc9   Thumb Code    22  irq_redirect .o(i.EXTI_INT4_IRQn_Handler)
    EXTI_INT5_IRQn_Handler                   0x00010be5   Thumb Code    22  irq_redirect .o(i.EXTI_INT5_IRQn_Handler)
    EXTI_INT6_IRQn_Handler                   0x00010c01   Thumb Code    22  irq_redirect .o(i.EXTI_INT6_IRQn_Handler)
    EXTI_INT7_IRQn_Handler                   0x00010c1d   Thumb Code    22  irq_redirect .o(i.EXTI_INT7_IRQn_Handler)
    FLSCTRL_IRQn_Handler                     0x00010c39   Thumb Code    14  irq_redirect .o(i.FLSCTRL_IRQn_Handler)
    Gpio_swire_output                        0x00010c4d   Thumb Code    78  ap_demo.o(i.Gpio_swire_output)
    HardFault_Handler                        0x00010c9d   Thumb Code    14  irq_redirect .o(i.HardFault_Handler)
    I2C0_IRQn_Handler                        0x00010cb1   Thumb Code    18  irq_redirect .o(i.I2C0_IRQn_Handler)
    I2C1_IRQn_Handler                        0x00010cc9   Thumb Code    18  irq_redirect .o(i.I2C1_IRQn_Handler)
    LCDC_IRQn_Handler                        0x00010ce1   Thumb Code    18  irq_redirect .o(i.LCDC_IRQn_Handler)
    LOG_printf                               0x00010cf9   Thumb Code    30  tau_log.o(i.LOG_printf)
    MEMC_IRQn_Handler                        0x00010d21   Thumb Code    18  irq_redirect .o(i.MEMC_IRQn_Handler)
    MIPI_RX_IRQn_Handler                     0x00010d39   Thumb Code    18  irq_redirect .o(i.MIPI_RX_IRQn_Handler)
    MIPI_TX_IRQn_Handler                     0x00010d51   Thumb Code    18  irq_redirect .o(i.MIPI_TX_IRQn_Handler)
    PWMDET_IRQn_Handler                      0x00010d69   Thumb Code    22  irq_redirect .o(i.PWMDET_IRQn_Handler)
    PWM_Task                                 0x00010d85   Thumb Code   112  ap_demo.o(i.PWM_Task)
    S20_Start_init                           0x00010e35   Thumb Code   282  app_tp_transfer.o(i.S20_Start_init)
    SPIM_IRQn_Handler                        0x00010f69   Thumb Code    22  irq_redirect .o(i.SPIM_IRQn_Handler)
    SPIS_IRQn_Handler                        0x00010f85   Thumb Code    22  irq_redirect .o(i.SPIS_IRQn_Handler)
    SWIRE_IRQn_Handler                       0x00010fa1   Thumb Code    22  irq_redirect .o(i.SWIRE_IRQn_Handler)
    SysTick_Handler                          0x00010fbd   Thumb Code    18  irq_redirect .o(i.SysTick_Handler)
    TIMER0_IRQn_Handler                      0x00010fd5   Thumb Code    18  irq_redirect .o(i.TIMER0_IRQn_Handler)
    UART_DisableDma                          0x00010fed   Thumb Code     2  drv_uart.o(i.UART_DisableDma)
    UART_GetInstance                         0x00010fef   Thumb Code     4  drv_uart.o(i.UART_GetInstance)
    __scatterload_copy                       0x00010ff3   Thumb Code    14  handlers.o(i.__scatterload_copy)
    s_RAM_CK                                 0x00011000   Data          20  drv_common.o(.ARM.__at_0x11000)
    TIMER1_IRQn_Handler                      0x00011015   Thumb Code    18  irq_redirect .o(i.TIMER1_IRQn_Handler)
    TIMER2_IRQn_Handler                      0x0001102d   Thumb Code    18  irq_redirect .o(i.TIMER2_IRQn_Handler)
    TIMER3_IRQn_Handler                      0x00011045   Thumb Code    18  irq_redirect .o(i.TIMER3_IRQn_Handler)
    UART0_IRQ_Handle                         0x0001105d   Thumb Code    20  drv_uart.o(i.UART0_IRQ_Handle)
    UART_IRQn_Handler                        0x00011079   Thumb Code    18  irq_redirect .o(i.UART_IRQn_Handler)
    UART_ResetRxFIFO                         0x00011091   Thumb Code    32  drv_uart.o(i.UART_ResetRxFIFO)
    UART_SetBaudRate                         0x000110b5   Thumb Code    72  drv_uart.o(i.UART_SetBaudRate)
    UART_SwitchSCLK                          0x000110fd   Thumb Code    26  drv_uart.o(i.UART_SwitchSCLK)
    UART_TransferHandleIRQ                   0x00011117   Thumb Code   308  drv_uart.o(i.UART_TransferHandleIRQ)
    UART_WriteBlocking                       0x0001124b   Thumb Code    26  drv_uart.o(i.UART_WriteBlocking)
    UART_init                                0x00011265   Thumb Code   182  drv_uart.o(i.UART_init)
    VIDC_IRQn_Handler                        0x00011321   Thumb Code    18  irq_redirect .o(i.VIDC_IRQn_Handler)
    VPRE_IRQn_Handler                        0x00011339   Thumb Code    18  irq_redirect .o(i.VPRE_IRQn_Handler)
    WDG_IRQn_Handler                         0x00011351   Thumb Code    18  irq_redirect .o(i.WDG_IRQn_Handler)
    __0printf                                0x00011369   Thumb Code    24  printfa.o(i.__0printf)
    __1printf                                0x00011369   Thumb Code     0  printfa.o(i.__0printf)
    __2printf                                0x00011369   Thumb Code     0  printfa.o(i.__0printf)
    __c89printf                              0x00011369   Thumb Code     0  printfa.o(i.__0printf)
    printf                                   0x00011369   Thumb Code     0  printfa.o(i.__0printf)
    __0vsprintf                              0x00011389   Thumb Code    30  printfa.o(i.__0vsprintf)
    __1vsprintf                              0x00011389   Thumb Code     0  printfa.o(i.__0vsprintf)
    __2vsprintf                              0x00011389   Thumb Code     0  printfa.o(i.__0vsprintf)
    __c89vsprintf                            0x00011389   Thumb Code     0  printfa.o(i.__0vsprintf)
    vsprintf                                 0x00011389   Thumb Code     0  printfa.o(i.__0vsprintf)
    __ARM_clz                                0x000113ad   Thumb Code    46  depilogue.o(i.__ARM_clz)
    __ARM_common_switch8                     0x000113db   Thumb Code    26  hal_dsi_rx_ctrl.o(i.__ARM_common_switch8)
    __scatterload_null                       0x000114b9   Thumb Code     2  handlers.o(i.__scatterload_null)
    __scatterload_zeroinit                   0x000114bb   Thumb Code    14  handlers.o(i.__scatterload_zeroinit)
    ap_demo                                  0x00012f05   Thumb Code   304  ap_demo.o(i.ap_demo)
    ap_tp_calibration                        0x00013415   Thumb Code   170  app_tp_transfer.o(i.ap_tp_calibration)
    app_ADC_IRQn_Handler                     0x000134c5   Thumb Code    22  drv_rxbr.o(i.app_ADC_IRQn_Handler)
    app_AP_NRESET_IRQn_Handler               0x000134e1   Thumb Code    32  drv_gpio.o(i.app_AP_NRESET_IRQn_Handler)
    app_EXTI_INT0_IRQn_Handler               0x00013505   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler)
    app_EXTI_INT1_IRQn_Handler               0x00013521   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler)
    app_EXTI_INT2_IRQn_Handler               0x0001353d   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler)
    app_EXTI_INT3_IRQn_Handler               0x00013559   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler)
    app_EXTI_INT4_IRQn_Handler               0x00013575   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler)
    app_EXTI_INT5_IRQn_Handler               0x00013591   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler)
    app_EXTI_INT6_IRQn_Handler               0x000135ad   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler)
    app_EXTI_INT7_IRQn_Handler               0x000135c9   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler)
    app_HardFault_Handler                    0x000135e5   Thumb Code    12  drv_common.o(i.app_HardFault_Handler)
    app_I2C0_IRQn_Handler                    0x0001362d   Thumb Code     8  drv_i2c_slave.o(i.app_I2C0_IRQn_Handler)
    app_I2C1_IRQn_Handler                    0x0001363d   Thumb Code     8  drv_i2c_master.o(i.app_I2C1_IRQn_Handler)
    app_LCDC_IRQn_Handler                    0x0001364d   Thumb Code    98  hal_internal_vsync.o(i.app_LCDC_IRQn_Handler)
    app_MEMC_IRQn_Handler                    0x0001372d   Thumb Code   132  drv_memc.o(i.app_MEMC_IRQn_Handler)
    app_MIPI_RX_IRQn_Handler                 0x000137b5   Thumb Code   228  drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler)
    app_MIPI_TX_IRQn_Handler                 0x00013a41   Thumb Code    56  drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler)
    app_PWMDET_IRQn_Handler                  0x00013ae1   Thumb Code    62  drv_pwm.o(i.app_PWMDET_IRQn_Handler)
    app_SPIM_IRQn_Handler                    0x00013b29   Thumb Code    34  drv_spi_master.o(i.app_SPIM_IRQn_Handler)
    app_SPIS_IRQn_Handler                    0x00013b59   Thumb Code   152  hal_spi_slave.o(i.app_SPIS_IRQn_Handler)
    app_SWIRE_IRQn_Handler                   0x00013bfd   Thumb Code    28  drv_swire.o(i.app_SWIRE_IRQn_Handler)
    app_SysTick_Handler                      0x00013c1d   Thumb Code    20  drv_common.o(i.app_SysTick_Handler)
    app_TIMER0_IRQn_Handler                  0x00013c35   Thumb Code    32  drv_timer.o(i.app_TIMER0_IRQn_Handler)
    app_TIMER1_IRQn_Handler                  0x00013c59   Thumb Code    32  drv_timer.o(i.app_TIMER1_IRQn_Handler)
    app_TIMER2_IRQn_Handler                  0x00013c7d   Thumb Code    32  drv_timer.o(i.app_TIMER2_IRQn_Handler)
    app_TIMER3_IRQn_Handler                  0x00013ca1   Thumb Code    48  drv_timer.o(i.app_TIMER3_IRQn_Handler)
    app_UART_IRQn_Handler                    0x00013cd5   Thumb Code     8  drv_uart.o(i.app_UART_IRQn_Handler)
    app_VIDC_IRQn_Handler                    0x00013cdd   Thumb Code    22  drv_vidc.o(i.app_VIDC_IRQn_Handler)
    app_VPRE_IRQn_Handler                    0x00013cf9   Thumb Code    22  drv_rxbr.o(i.app_VPRE_IRQn_Handler)
    app_WDG_IRQn_Handler                     0x00013d15   Thumb Code    40  drv_wdg.o(i.app_WDG_IRQn_Handler)
    app_dma_irq_handler                      0x00013d41   Thumb Code    10  drv_dma.o(i.app_dma_irq_handler)
    app_fls_ctrl_Handler                     0x00013d51   Thumb Code    38  norflash.o(i.app_fls_ctrl_Handler)
    app_tp_I2C_init                          0x00013d81   Thumb Code    26  app_tp_transfer.o(i.app_tp_I2C_init)
    app_tp_calibration_exec                  0x00013da5   Thumb Code    30  ap_demo.o(i.app_tp_calibration_exec)
    app_tp_init                              0x00013e31   Thumb Code    58  app_tp_transfer.o(i.app_tp_init)
    app_tp_phone_analysis_data               0x00013ea1   Thumb Code   770  app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data)
    app_tp_phone_clear_reset_on              0x000141b9   Thumb Code     8  app_tp_transfer.o(i.app_tp_phone_clear_reset_on)
    app_tp_s_read                            0x000141c5   Thumb Code     8  app_tp_transfer.o(i.app_tp_s_read)
    app_tp_s_write                           0x000141cd   Thumb Code     8  app_tp_transfer.o(i.app_tp_s_write)
    app_tp_screen_analysis_int               0x000141d5   Thumb Code   658  app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int)
    app_tp_screen_init                       0x00014471   Thumb Code    42  app_tp_transfer.o(i.app_tp_screen_init)
    app_tp_transfer_screen_int               0x000144ed   Thumb Code   218  app_tp_transfer.o(i.app_tp_transfer_screen_int)
    app_tp_transfer_screen_start             0x000145d9   Thumb Code    18  app_tp_transfer.o(i.app_tp_transfer_screen_start)
    board_Init                               0x000145f1   Thumb Code    24  board.o(i.board_Init)
    ceil                                     0x000148c1   Thumb Code   180  ceil.o(i.ceil)
    dcs_packet_fifo_alloc                    0x00014a45   Thumb Code    80  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    dcs_packet_fifo_init                     0x00014a9d   Thumb Code    18  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    dcs_packet_free_fifo_header              0x00014ab5   Thumb Code    60  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    dcs_packet_get_fifo_header               0x00014af9   Thumb Code    26  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    delayMs                                  0x00014b39   Thumb Code    24  tau_delay.o(i.delayMs)
    delayUs                                  0x00014b51   Thumb Code    34  tau_delay.o(i.delayUs)
    drv_ap_rst_trig_edge_detect              0x00014b75   Thumb Code    46  drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect)
    drv_chip_info_get_info                   0x00014bad   Thumb Code     6  drv_chip_info.o(i.drv_chip_info_get_info)
    drv_chip_info_init                       0x00014bb9   Thumb Code    56  drv_chip_info.o(i.drv_chip_info_init)
    drv_chip_rx_info_check                   0x00014bf9   Thumb Code   122  drv_chip_info.o(i.drv_chip_rx_info_check)
    drv_chip_rx_init_done                    0x00014cc1   Thumb Code    16  drv_chip_info.o(i.drv_chip_rx_init_done)
    drv_common_enable_systick                0x00014cd5   Thumb Code    70  drv_common.o(i.drv_common_enable_systick)
    drv_common_system_init                   0x00014d2d   Thumb Code     8  drv_common.o(i.drv_common_system_init)
    drv_crgu_clear_all_reset_flags           0x00014d35   Thumb Code     8  drv_crgu.o(i.drv_crgu_clear_all_reset_flags)
    drv_crgu_config_reset_modules            0x00014d41   Thumb Code    10  drv_crgu.o(i.drv_crgu_config_reset_modules)
    drv_crgu_set_ahb_pre_div                 0x00014d51   Thumb Code    14  drv_crgu.o(i.drv_crgu_set_ahb_pre_div)
    drv_crgu_set_ahb_src                     0x00014d65   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_ahb_src)
    drv_crgu_set_clock                       0x00014d79   Thumb Code    26  drv_crgu.o(i.drv_crgu_set_clock)
    drv_crgu_set_dpi_mux_src                 0x00014d99   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dpi_mux_src)
    drv_crgu_set_dpi_pre_div                 0x00014dad   Thumb Code    18  drv_crgu.o(i.drv_crgu_set_dpi_pre_div)
    drv_crgu_set_dpi_pre_src                 0x00014dc5   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dpi_pre_src)
    drv_crgu_set_dsc_core_div                0x00014dd9   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dsc_core_div)
    drv_crgu_set_dsco_src                    0x00014ded   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dsco_src)
    drv_crgu_set_dsco_src_div                0x00014e01   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dsco_src_div)
    drv_crgu_set_fb_div                      0x00014e15   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_fb_div)
    drv_crgu_set_fb_src                      0x00014e29   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_fb_src)
    drv_crgu_set_lcdc_div                    0x00014e3d   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_lcdc_div)
    drv_crgu_set_lcdc_src                    0x00014e51   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_lcdc_src)
    drv_crgu_set_mipi_cfg_src                0x00014e65   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_mipi_cfg_src)
    drv_crgu_set_mipi_ref_src                0x00014e79   Thumb Code    18  drv_crgu.o(i.drv_crgu_set_mipi_ref_src)
    drv_crgu_set_reset                       0x00014e91   Thumb Code    20  drv_crgu.o(i.drv_crgu_set_reset)
    drv_crgu_set_rxbr_div                    0x00014ea9   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_rxbr_div)
    drv_crgu_set_rxbr_src                    0x00014ebd   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_rxbr_src)
    drv_crgu_set_vidc_src                    0x00014ed1   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_vidc_src)
    drv_dma_clear_flag                       0x00014ee5   Thumb Code    24  drv_dma.o(i.drv_dma_clear_flag)
    drv_dma_create_handle                    0x00014efd   Thumb Code    22  drv_dma.o(i.drv_dma_create_handle)
    drv_dma_disenable_channel                0x00014f19   Thumb Code    16  drv_dma.o(i.drv_dma_disenable_channel)
    drv_dma_enable_channel                   0x00014f29   Thumb Code    16  drv_dma.o(i.drv_dma_enable_channel)
    drv_dma_enable_channel_interrupts        0x00014f39   Thumb Code    32  drv_dma.o(i.drv_dma_enable_channel_interrupts)
    drv_dma_get_channel_flag                 0x00014f5d   Thumb Code    12  drv_dma.o(i.drv_dma_get_channel_flag)
    drv_dma_irq_handler                      0x00014f69   Thumb Code   138  drv_dma.o(i.drv_dma_irq_handler)
    drv_dma_prepar_transfer                  0x00014ff9   Thumb Code    18  drv_dma.o(i.drv_dma_prepar_transfer)
    drv_dma_set_burst                        0x0001500b   Thumb Code    26  drv_dma.o(i.drv_dma_set_burst)
    drv_dma_set_callback                     0x00015025   Thumb Code     6  drv_dma.o(i.drv_dma_set_callback)
    drv_dma_set_transfer                     0x0001502d   Thumb Code    62  drv_dma.o(i.drv_dma_set_transfer)
    drv_dsc_dec_convert_pps_rc_parameter     0x00015071   Thumb Code    54  drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter)
    drv_dsc_dec_disable                      0x000150a7   Thumb Code    12  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    drv_dsc_dec_enable                       0x000150b5   Thumb Code    88  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    drv_dsc_dec_get_nslc                     0x00015129   Thumb Code    10  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    drv_dsc_dec_set_u8_pps                   0x00015133   Thumb Code    40  drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps)
    drv_dsi_rx_calc_ipi_tx_delay             0x0001515d   Thumb Code   244  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    drv_dsi_rx_enable_irq                    0x00015261   Thumb Code    58  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    drv_dsi_rx_get_compression_en            0x0001530d   Thumb Code     8  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    drv_dsi_rx_get_max_ret_size              0x00015315   Thumb Code     6  drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size)
    drv_dsi_rx_power_up                      0x0001531b   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    drv_dsi_rx_set_ctrl_cfg                  0x00015329   Thumb Code    32  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    drv_dsi_rx_set_ddi_cfg                   0x00015349   Thumb Code    16  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    drv_dsi_rx_set_inten                     0x00015359   Thumb Code     4  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    drv_dsi_rx_set_ipi_cfg                   0x0001535d   Thumb Code    16  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    drv_dsi_rx_set_lane_swap                 0x0001536d   Thumb Code    70  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    drv_dsi_rx_set_up_phy                    0x000153b5   Thumb Code   202  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    drv_dsi_rx_shut_down                     0x00015485   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    drv_dsi_tx_command_header                0x00015493   Thumb Code    20  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    drv_dsi_tx_command_mode_cfg              0x000154a7   Thumb Code   108  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    drv_dsi_tx_command_put_payload           0x00015513   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    drv_dsi_tx_config_eotp                   0x00015517   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    drv_dsi_tx_config_int                    0x0001552f   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    drv_dsi_tx_dpi_lpcmd_time                0x00015537   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    drv_dsi_tx_dpi_mode                      0x0001553f   Thumb Code    10  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    drv_dsi_tx_dpi_polarity                  0x00015549   Thumb Code    36  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    drv_dsi_tx_edpi_cmd_size                 0x0001556d   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    drv_dsi_tx_get_cmd_status                0x00015571   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    drv_dsi_tx_mode                          0x00015575   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    drv_dsi_tx_phy_clock_lane_auto_lp        0x00015579   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    drv_dsi_tx_phy_clock_lane_req_hs         0x00015591   Thumb Code    26  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    drv_dsi_tx_phy_lane_mode                 0x000155ab   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    drv_dsi_tx_phy_status_ready              0x000155b7   Thumb Code   100  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    drv_dsi_tx_phy_status_stopstate          0x0001561b   Thumb Code    62  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    drv_dsi_tx_phy_time_cfg                  0x00015659   Thumb Code    30  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    drv_dsi_tx_powerup                       0x00015677   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    drv_dsi_tx_response_mode                 0x0001567f   Thumb Code    28  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    drv_dsi_tx_set_bta_ack                   0x0001569b   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    drv_dsi_tx_set_esc_div                   0x000156b3   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    drv_dsi_tx_set_int                       0x000156c1   Thumb Code    46  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    drv_dsi_tx_set_time_out_div              0x000156f5   Thumb Code    16  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    drv_dsi_tx_set_video_chunk               0x00015705   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    drv_dsi_tx_set_video_timing              0x0001570d   Thumb Code    34  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    drv_dsi_tx_shutdown                      0x0001572f   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    drv_dsi_tx_timeout_cfg                   0x00015737   Thumb Code    38  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    drv_dsi_tx_video_mode_cfg                0x0001575d   Thumb Code   170  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    drv_dsi_tx_video_mode_disable_hact_cmd   0x00015807   Thumb Code    22  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_disable_hact_cmd)
    drv_dsi_tx_video_mode_set_lp_cmd         0x0001581d   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd)
    drv_efuse_enter_inactive                 0x00015835   Thumb Code    32  drv_efuse.o(i.drv_efuse_enter_inactive)
    drv_efuse_int_enable                     0x00015855   Thumb Code    12  drv_efuse.o(i.drv_efuse_int_enable)
    drv_efuse_read                           0x00015861   Thumb Code    50  drv_efuse.o(i.drv_efuse_read)
    drv_efuse_read_req                       0x00015893   Thumb Code    24  drv_efuse.o(i.drv_efuse_read_req)
    drv_gpio_get_input_data                  0x000158ad   Thumb Code    20  drv_gpio.o(i.drv_gpio_get_input_data)
    drv_gpio_register_ap_reset_callback      0x000158c5   Thumb Code     6  drv_gpio.o(i.drv_gpio_register_ap_reset_callback)
    drv_gpio_register_callback               0x000158d1   Thumb Code    14  drv_gpio.o(i.drv_gpio_register_callback)
    drv_gpio_set_int                         0x000158e5   Thumb Code    62  drv_gpio.o(i.drv_gpio_set_int)
    drv_gpio_set_ioe                         0x00015929   Thumb Code    26  drv_gpio.o(i.drv_gpio_set_ioe)
    drv_gpio_set_mode0                       0x00015949   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode0)
    drv_gpio_set_mode1                       0x00015959   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode1)
    drv_gpio_set_mode2                       0x00015969   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode2)
    drv_gpio_set_mode3                       0x00015979   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode3)
    drv_gpio_set_pull_state                  0x000159a9   Thumb Code   298  drv_gpio.o(i.drv_gpio_set_pull_state)
    drv_i2c_dma_init                         0x00015b0d   Thumb Code   146  drv_i2c_dma.o(i.drv_i2c_dma_init)
    drv_i2c_enable_rx_dma                    0x00015bb9   Thumb Code    26  drv_i2c_dma.o(i.drv_i2c_enable_rx_dma)
    drv_i2c_enable_tx_dma                    0x00015bd3   Thumb Code    24  drv_i2c_dma.o(i.drv_i2c_enable_tx_dma)
    drv_i2c_m_clear_it_pending_bit           0x00015bed   Thumb Code    86  drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit)
    drv_i2c_m_enable                         0x00015c4d   Thumb Code    10  drv_i2c_master.o(i.drv_i2c_m_enable)
    drv_i2c_m_enable_intr                    0x00015c5d   Thumb Code    42  drv_i2c_master.o(i.drv_i2c_m_enable_intr)
    drv_i2c_m_set_callback                   0x00015c95   Thumb Code     6  drv_i2c_master.o(i.drv_i2c_m_set_callback)
    drv_i2c_master_init                      0x00015ca1   Thumb Code   118  drv_i2c_master.o(i.drv_i2c_master_init)
    drv_i2c_master_read_dma                  0x00015d2d   Thumb Code    82  drv_i2c_dma.o(i.drv_i2c_master_read_dma)
    drv_i2c_master_write_dma                 0x00015d89   Thumb Code    50  drv_i2c_dma.o(i.drv_i2c_master_write_dma)
    drv_i2c_s_clear_it_pending_bit           0x00015df5   Thumb Code    84  drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit)
    drv_i2c_s_enable_intr                    0x00015e51   Thumb Code    40  drv_i2c_slave.o(i.drv_i2c_s_enable_intr)
    drv_i2c_s_get_fifo_status                0x00015e85   Thumb Code    22  drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status)
    drv_i2c_s_set_callback                   0x00015ea1   Thumb Code     6  drv_i2c_slave.o(i.drv_i2c_s_set_callback)
    drv_i2c_s_write_data                     0x00015ead   Thumb Code    26  drv_i2c_slave.o(i.drv_i2c_s_write_data)
    drv_i2c_set_dma_irq_callback             0x00015ecd   Thumb Code    68  drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback)
    drv_i2c_slave_init                       0x00015f25   Thumb Code    60  drv_i2c_slave.o(i.drv_i2c_slave_init)
    drv_i2c_slave_write_dma                  0x00015f69   Thumb Code    18  drv_i2c_dma.o(i.drv_i2c_slave_write_dma)
    drv_lcdc_config_bypass                   0x00015f85   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_config_bypass)
    drv_lcdc_config_ccm                      0x00015f9d   Thumb Code    48  drv_lcdc.o(i.drv_lcdc_config_ccm)
    drv_lcdc_config_disp_mode                0x00015fcd   Thumb Code    22  drv_lcdc.o(i.drv_lcdc_config_disp_mode)
    drv_lcdc_config_dpi_polarity             0x00015fe3   Thumb Code    36  drv_lcdc.o(i.drv_lcdc_config_dpi_polarity)
    drv_lcdc_config_dpi_timing               0x00016007   Thumb Code    38  drv_lcdc.o(i.drv_lcdc_config_dpi_timing)
    drv_lcdc_config_edpi_mode                0x0001602d   Thumb Code    22  drv_lcdc.o(i.drv_lcdc_config_edpi_mode)
    drv_lcdc_config_endianness               0x00016043   Thumb Code    22  drv_lcdc.o(i.drv_lcdc_config_endianness)
    drv_lcdc_config_input_size               0x00016059   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_config_input_size)
    drv_lcdc_config_int                      0x00016065   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_config_int)
    drv_lcdc_config_int_single               0x00016083   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_int_single)
    drv_lcdc_config_overwrite                0x000160a5   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_overwrite)
    drv_lcdc_config_overwrite_rgb            0x000160c7   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    drv_lcdc_config_partial_display_area     0x000160d3   Thumb Code    26  drv_lcdc.o(i.drv_lcdc_config_partial_display_area)
    drv_lcdc_config_partial_display_enable   0x000160ed   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_partial_display_enable)
    drv_lcdc_config_scale_up_coef            0x0001610f   Thumb Code    40  drv_lcdc.o(i.drv_lcdc_config_scale_up_coef)
    drv_lcdc_config_scale_up_step            0x00016137   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_config_scale_up_step)
    drv_lcdc_config_src_parameter            0x00016143   Thumb Code    76  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    drv_lcdc_config_thresh                   0x0001618f   Thumb Code     6  drv_lcdc.o(i.drv_lcdc_config_thresh)
    drv_lcdc_ctrl_flow                       0x00016195   Thumb Code    18  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    drv_lcdc_enable_shadow_reg               0x000161a7   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    drv_lcdc_set_int                         0x000161c9   Thumb Code    46  drv_lcdc.o(i.drv_lcdc_set_int)
    drv_lcdc_set_video_hw_mode               0x000161fd   Thumb Code    20  drv_lcdc.o(i.drv_lcdc_set_video_hw_mode)
    drv_lcdc_start                           0x00016211   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_start)
    drv_memc_clear_status                    0x00016231   Thumb Code    12  drv_memc.o(i.drv_memc_clear_status)
    drv_memc_enable_irq                      0x0001623d   Thumb Code    58  drv_memc.o(i.drv_memc_enable_irq)
    drv_memc_gen_a_tear_signal               0x0001627d   Thumb Code    12  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    drv_memc_get_status                      0x00016289   Thumb Code    18  drv_memc.o(i.drv_memc_get_status)
    drv_memc_rate_transfer_sel               0x0001629b   Thumb Code    16  drv_memc.o(i.drv_memc_rate_transfer_sel)
    drv_memc_sel_vsync                       0x000162ab   Thumb Code    14  drv_memc.o(i.drv_memc_sel_vsync)
    drv_memc_set_active_height               0x000162b9   Thumb Code    14  drv_memc.o(i.drv_memc_set_active_height)
    drv_memc_set_data_mode                   0x000162cd   Thumb Code    12  drv_memc.o(i.drv_memc_set_data_mode)
    drv_memc_set_double_buffer               0x000162d9   Thumb Code    16  drv_memc.o(i.drv_memc_set_double_buffer)
    drv_memc_set_double_buffer_reverse       0x000162e9   Thumb Code    18  drv_memc.o(i.drv_memc_set_double_buffer_reverse)
    drv_memc_set_fs_en_conditions            0x000162fb   Thumb Code    16  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    drv_memc_set_inten                       0x0001630b   Thumb Code    20  drv_memc.o(i.drv_memc_set_inten)
    drv_memc_set_lcdc_st_conditions          0x00016321   Thumb Code    18  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    drv_memc_set_ltpo_mode                   0x00016339   Thumb Code    26  drv_memc.o(i.drv_memc_set_ltpo_mode)
    drv_memc_set_tear_mode                   0x00016353   Thumb Code    14  drv_memc.o(i.drv_memc_set_tear_mode)
    drv_memc_set_tear_waveform               0x00016361   Thumb Code    34  drv_memc.o(i.drv_memc_set_tear_waveform)
    drv_memc_set_vidc_sync_cnt               0x00016389   Thumb Code    14  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    drv_param_init_get_ccm                   0x00016399   Thumb Code     4  drv_param_init.o(i.drv_param_init_get_ccm)
    drv_param_init_get_scld_filter_h         0x000163a1   Thumb Code    12  drv_param_init.o(i.drv_param_init_get_scld_filter_h)
    drv_param_init_get_scld_filter_v         0x000163b5   Thumb Code    12  drv_param_init.o(i.drv_param_init_get_scld_filter_v)
    drv_param_init_get_sclu_filter           0x000163c9   Thumb Code     4  drv_param_init.o(i.drv_param_init_get_sclu_filter)
    drv_param_init_set_ccm                   0x000163d1   Thumb Code    14  drv_param_init.o(i.drv_param_init_set_ccm)
    drv_param_p2r_filter_init                0x000163e5   Thumb Code    30  drv_param_init.o(i.drv_param_p2r_filter_init)
    drv_phy_get_para                         0x00016409   Thumb Code    76  drv_phy_common.o(i.drv_phy_get_para)
    drv_pwm_out_enable                       0x0001645d   Thumb Code    26  drv_pwm.o(i.drv_pwm_out_enable)
    drv_pwm_out_set_control                  0x0001647d   Thumb Code     6  drv_pwm.o(i.drv_pwm_out_set_control)
    drv_pwm_out_set_period                   0x00016489   Thumb Code     6  drv_pwm.o(i.drv_pwm_out_set_period)
    drv_pwm_out_set_threshold                0x00016495   Thumb Code     8  drv_pwm.o(i.drv_pwm_out_set_threshold)
    drv_pwr_set_cp_mode                      0x000164a1   Thumb Code    26  drv_pwr.o(i.drv_pwr_set_cp_mode)
    drv_pwr_set_pvd_mode                     0x000164c1   Thumb Code    18  drv_pwr.o(i.drv_pwr_set_pvd_mode)
    drv_pwr_set_system_clk_src               0x000164d9   Thumb Code    36  drv_pwr.o(i.drv_pwr_set_system_clk_src)
    drv_rxbr_clear_pkt_buffer                0x000165a5   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    drv_rxbr_clear_status0                   0x000165af   Thumb Code     4  drv_rxbr.o(i.drv_rxbr_clear_status0)
    drv_rxbr_enable_irq                      0x000165b3   Thumb Code    90  drv_rxbr.o(i.drv_rxbr_enable_irq)
    drv_rxbr_frame_drop_cfg                  0x0001660d   Thumb Code    16  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    drv_rxbr_get_clk                         0x00016621   Thumb Code    44  drv_rxbr.o(i.drv_rxbr_get_clk)
    drv_rxbr_get_col_addr                    0x0001665d   Thumb Code     4  drv_rxbr.o(i.drv_rxbr_get_col_addr)
    drv_rxbr_get_page_addr                   0x00016673   Thumb Code     4  drv_rxbr.o(i.drv_rxbr_get_page_addr)
    drv_rxbr_hline_rcv0_cfg                  0x00016689   Thumb Code    12  drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg)
    drv_rxbr_hline_rcv_cfg                   0x00016695   Thumb Code     8  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    drv_rxbr_register_irq0_callback          0x0001669d   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_register_irq0_callback)
    drv_rxbr_register_irq1_callback          0x000166a9   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    drv_rxbr_set_ack_pkt_header              0x000166b5   Thumb Code    20  drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header)
    drv_rxbr_set_cmd_filter                  0x000166c9   Thumb Code   204  drv_rxbr.o(i.drv_rxbr_set_cmd_filter)
    drv_rxbr_set_color_format                0x00016795   Thumb Code    20  drv_rxbr.o(i.drv_rxbr_set_color_format)
    drv_rxbr_set_inten                       0x000167a9   Thumb Code    20  drv_rxbr.o(i.drv_rxbr_set_inten)
    drv_rxbr_set_ltpo_drop_th                0x000167bd   Thumb Code    16  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    drv_rxbr_set_usr_cfg                     0x000167cd   Thumb Code    38  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    drv_rxbr_set_usr_col                     0x000167f3   Thumb Code     8  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    drv_rxbr_set_usr_row                     0x000167fb   Thumb Code     8  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    drv_spi_m_read_data                      0x00016805   Thumb Code    28  drv_spi_master.o(i.drv_spi_m_read_data)
    drv_swire_set_int                        0x00016825   Thumb Code    64  drv_swire.o(i.drv_swire_set_int)
    drv_swire_set_power_down                 0x0001686d   Thumb Code    24  drv_swire.o(i.drv_swire_set_power_down)
    drv_sys_cfg_clear_all_int                0x00016889   Thumb Code     8  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    drv_sys_cfg_clear_pending                0x00016895   Thumb Code    32  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    drv_sys_cfg_sel_ap_rst_lvl_trig          0x000168bd   Thumb Code    18  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig)
    drv_sys_cfg_sel_ap_rst_trig              0x000168d5   Thumb Code    22  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig)
    drv_sys_cfg_sel_gpio_group               0x000168f1   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group)
    drv_sys_cfg_sel_int_trig                 0x00016915   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig)
    drv_sys_cfg_set_dma_rx_req               0x00016939   Thumb Code    10  drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req)
    drv_sys_cfg_set_dma_tx_req               0x00016949   Thumb Code    10  drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req)
    drv_sys_cfg_set_int                      0x00016959   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    drv_timer_clear_status_flags             0x0001697d   Thumb Code    26  drv_timer.o(i.drv_timer_clear_status_flags)
    drv_timer_enable                         0x00016997   Thumb Code    32  drv_timer.o(i.drv_timer_enable)
    drv_timer_get_instance                   0x000169b9   Thumb Code     8  drv_timer.o(i.drv_timer_get_instance)
    drv_timer_get_prescaler                  0x000169c5   Thumb Code    14  drv_timer.o(i.drv_timer_get_prescaler)
    drv_timer_register_callback              0x000169d5   Thumb Code    12  drv_timer.o(i.drv_timer_register_callback)
    drv_timer_set_current_count              0x000169e5   Thumb Code    12  drv_timer.o(i.drv_timer_set_current_count)
    drv_timer_set_int                        0x000169f1   Thumb Code    68  drv_timer.o(i.drv_timer_set_int)
    drv_timer_set_match                      0x00016a39   Thumb Code    12  drv_timer.o(i.drv_timer_set_match)
    drv_timer_set_prescaler                  0x00016a45   Thumb Code    22  drv_timer.o(i.drv_timer_set_prescaler)
    drv_tx_phy_test_clear                    0x00016a5b   Thumb Code    12  drv_dsi_tx.o(i.drv_tx_phy_test_clear)
    drv_tx_phy_test_enter                    0x00016a67   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    drv_tx_phy_test_exit                     0x00016a83   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    drv_tx_phy_test_write                    0x00016a9f   Thumb Code    26  drv_dsi_tx.o(i.drv_tx_phy_test_write)
    drv_tx_phy_test_write_1_byte             0x00016ab9   Thumb Code    14  drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte)
    drv_tx_phy_test_write_2_byte             0x00016ac7   Thumb Code    18  drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte)
    drv_tx_phy_test_write_code               0x00016ad9   Thumb Code    34  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    drv_vidc_clear_irq                       0x00016b1d   Thumb Code     8  drv_vidc.o(i.drv_vidc_clear_irq)
    drv_vidc_enable                          0x00016b25   Thumb Code    24  drv_vidc.o(i.drv_vidc_enable)
    drv_vidc_enable_irq                      0x00016b3d   Thumb Code    58  drv_vidc.o(i.drv_vidc_enable_irq)
    drv_vidc_get_irq_status                  0x00016b7d   Thumb Code    18  drv_vidc.o(i.drv_vidc_get_irq_status)
    drv_vidc_init_module_enable              0x00016b91   Thumb Code    36  drv_vidc.o(i.drv_vidc_init_module_enable)
    drv_vidc_register_callback               0x00016bb9   Thumb Code     6  drv_vidc.o(i.drv_vidc_register_callback)
    drv_vidc_reset                           0x00016bc5   Thumb Code     6  drv_vidc.o(i.drv_vidc_reset)
    drv_vidc_set_dst_parameter               0x00016bcb   Thumb Code    60  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    drv_vidc_set_irqen                       0x00016c07   Thumb Code    20  drv_vidc.o(i.drv_vidc_set_irqen)
    drv_vidc_set_mirror                      0x00016c1b   Thumb Code    16  drv_vidc.o(i.drv_vidc_set_mirror)
    drv_vidc_set_p2r_hcoef0                  0x00016c2b   Thumb Code     8  drv_vidc.o(i.drv_vidc_set_p2r_hcoef0)
    drv_vidc_set_p2r_hinitb                  0x00016c33   Thumb Code    38  drv_vidc.o(i.drv_vidc_set_p2r_hinitb)
    drv_vidc_set_p2r_hinitr                  0x00016c59   Thumb Code    38  drv_vidc.o(i.drv_vidc_set_p2r_hinitr)
    drv_vidc_set_pentile_swap                0x00016c81   Thumb Code    18  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    drv_vidc_set_pu_ctrl                     0x00016c99   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    drv_vidc_set_rotation                    0x00016ca3   Thumb Code    16  drv_vidc.o(i.drv_vidc_set_rotation)
    drv_vidc_set_scld_hcoef0                 0x00016cb3   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    drv_vidc_set_scld_hcoef1                 0x00016cbd   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    drv_vidc_set_scld_step                   0x00016cc7   Thumb Code    18  drv_vidc.o(i.drv_vidc_set_scld_step)
    drv_vidc_set_scld_vcoef0                 0x00016cd9   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    drv_vidc_set_scld_vcoef1                 0x00016ce3   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    drv_vidc_set_src_parameter               0x00016ced   Thumb Code    22  drv_vidc.o(i.drv_vidc_set_src_parameter)
    drv_wdg_set_int                          0x00016d25   Thumb Code    48  drv_wdg.o(i.drv_wdg_set_int)
    fls_clr_interrupt_flag                   0x00016d59   Thumb Code    10  drv_fls.o(i.fls_clr_interrupt_flag)
    fputc                                    0x00016d63   Thumb Code    20  tau_log.o(i.fputc)
    hal_dsi_rx_ctrl_create_handle            0x00016d79   Thumb Code    42  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    hal_dsi_rx_ctrl_deinit                   0x00016da9   Thumb Code    32  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit)
    hal_dsi_rx_ctrl_dsc_async_handler        0x00016dcd   Thumb Code   120  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler)
    hal_dsi_rx_ctrl_gen_a_tear_signal        0x00016e51   Thumb Code    32  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal)
    hal_dsi_rx_ctrl_get_max_ret_size         0x00016e79   Thumb Code    30  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size)
    hal_dsi_rx_ctrl_init                     0x00016ea1   Thumb Code   144  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    hal_dsi_rx_ctrl_pre_init_pps             0x0001774d   Thumb Code    56  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    hal_dsi_rx_ctrl_send_ack_cmd             0x00017789   Thumb Code   212  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd)
    hal_dsi_rx_ctrl_set_cus_esc_clk          0x00017879   Thumb Code    34  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk)
    hal_dsi_rx_ctrl_set_cus_sync_line        0x000178a5   Thumb Code    44  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line)
    hal_dsi_rx_ctrl_set_hw_tear_mode         0x000178d9   Thumb Code    42  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode)
    hal_dsi_rx_ctrl_set_sw_tear_mode         0x0001790d   Thumb Code    42  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode)
    hal_dsi_rx_ctrl_start                    0x00017941   Thumb Code    46  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    hal_dsi_rx_ctrl_stop                     0x0001797d   Thumb Code    46  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop)
    hal_dsi_rx_ctrl_toggle_resolution        0x000179b9   Thumb Code    28  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    hal_dsi_tx_ctrl_create_handle            0x00018075   Thumb Code    34  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    hal_dsi_tx_ctrl_deinit                   0x000180a1   Thumb Code    68  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit)
    hal_dsi_tx_ctrl_enter_init_panel_mode    0x000180e9   Thumb Code    68  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode)
    hal_dsi_tx_ctrl_exit_init_panel_mode     0x00018135   Thumb Code    32  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode)
    hal_dsi_tx_ctrl_init                     0x0001815d   Thumb Code   154  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    hal_dsi_tx_ctrl_panel_reset_pin          0x00018225   Thumb Code    12  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin)
    hal_dsi_tx_ctrl_set_ccm                  0x00018231   Thumb Code    28  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm)
    hal_dsi_tx_ctrl_set_overwrite_rgb        0x00018251   Thumb Code    16  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    hal_dsi_tx_ctrl_set_partial_disp         0x00018265   Thumb Code    12  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp)
    hal_dsi_tx_ctrl_set_partial_disp_area    0x00018275   Thumb Code    30  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area)
    hal_dsi_tx_ctrl_start                    0x00018299   Thumb Code    94  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    hal_dsi_tx_ctrl_stop                     0x00018305   Thumb Code    54  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop)
    hal_dsi_tx_ctrl_write_array_cmd          0x00018349   Thumb Code   210  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd)
    hal_dsi_tx_ctrl_write_cmd                0x00018421   Thumb Code   172  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    hal_gpio_ctrl_eint                       0x00018819   Thumb Code    18  hal_gpio.o(i.hal_gpio_ctrl_eint)
    hal_gpio_get_input_data                  0x00018831   Thumb Code    18  hal_gpio.o(i.hal_gpio_get_input_data)
    hal_gpio_init_eint                       0x00018845   Thumb Code    58  hal_gpio.o(i.hal_gpio_init_eint)
    hal_gpio_init_output                     0x00018885   Thumb Code    34  hal_gpio.o(i.hal_gpio_init_output)
    hal_gpio_reg_eint_cb                     0x000188ad   Thumb Code    20  hal_gpio.o(i.hal_gpio_reg_eint_cb)
    hal_gpio_set_ap_reset_int                0x000188c5   Thumb Code    76  hal_gpio.o(i.hal_gpio_set_ap_reset_int)
    hal_gpio_set_mode                        0x00018915   Thumb Code    90  hal_gpio.o(i.hal_gpio_set_mode)
    hal_gpio_set_output_data                 0x00018975   Thumb Code     8  hal_gpio.o(i.hal_gpio_set_output_data)
    hal_gpio_set_pull_state                  0x0001897d   Thumb Code    26  hal_gpio.o(i.hal_gpio_set_pull_state)
    hal_i2c_m_dma_init                       0x0001899d   Thumb Code    92  hal_i2c_master.o(i.hal_i2c_m_dma_init)
    hal_i2c_m_dma_read                       0x00018a09   Thumb Code    26  hal_i2c_master.o(i.hal_i2c_m_dma_read)
    hal_i2c_m_dma_write                      0x00018a29   Thumb Code    24  hal_i2c_master.o(i.hal_i2c_m_dma_write)
    hal_i2c_m_transfer_complate              0x00018a45   Thumb Code     6  hal_i2c_master.o(i.hal_i2c_m_transfer_complate)
    hal_i2c_s_dma_write                      0x00018a81   Thumb Code    46  hal_i2c_slave.o(i.hal_i2c_s_dma_write)
    hal_i2c_s_init                           0x00018ab9   Thumb Code    86  hal_i2c_slave.o(i.hal_i2c_s_init)
    hal_i2c_s_nonblocking_read               0x00018b25   Thumb Code    14  hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read)
    hal_i2c_s_set_transfer                   0x00018b39   Thumb Code     6  hal_i2c_slave.o(i.hal_i2c_s_set_transfer)
    hal_internal_init_memc                   0x00018c5d   Thumb Code   146  hal_internal_vsync.o(i.hal_internal_init_memc)
    hal_internal_sync_get_fb_setting         0x00018d41   Thumb Code    12  hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting)
    hal_internal_sync_input_resolution_change 0x00018d51   Thumb Code   418  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    hal_internal_vsync_deinit                0x00018f65   Thumb Code    24  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    hal_internal_vsync_get_sync_line         0x00018f81   Thumb Code    18  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    hal_internal_vsync_init_rx               0x00018f99   Thumb Code   220  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    hal_internal_vsync_init_tx               0x00019095   Thumb Code   172  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    hal_internal_vsync_set_auto_hw_filter    0x00019145   Thumb Code   222  hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter)
    hal_internal_vsync_set_rx_state          0x00019261   Thumb Code    16  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    hal_internal_vsync_set_sync_line         0x00019275   Thumb Code    22  hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line)
    hal_internal_vsync_set_tear_mode         0x00019291   Thumb Code    58  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    hal_internal_vsync_set_tx_state          0x000192d5   Thumb Code    54  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    hal_pwm_out_config_all                   0x000196ad   Thumb Code   100  hal_pwm.o(i.hal_pwm_out_config_all)
    hal_pwm_out_init                         0x00019715   Thumb Code    12  hal_pwm.o(i.hal_pwm_out_init)
    hal_spi_m_clear_rxfifo                   0x00019721   Thumb Code    14  hal_spi_master.o(i.hal_spi_m_clear_rxfifo)
    hal_swire_open                           0x0001972f   Thumb Code    22  hal_swire.o(i.hal_swire_open)
    hal_system_enable_systick                0x00019745   Thumb Code     8  hal_system.o(i.hal_system_enable_systick)
    hal_system_init                          0x0001974d   Thumb Code    96  hal_system.o(i.hal_system_init)
    hal_system_init_console                  0x000197c9   Thumb Code    28  hal_system.o(i.hal_system_init_console)
    hal_system_set_pvd                       0x000197e5   Thumb Code     8  hal_system.o(i.hal_system_set_pvd)
    hal_system_set_vcc                       0x000197ed   Thumb Code     8  hal_system.o(i.hal_system_set_vcc)
    hal_timer_init                           0x000197f5   Thumb Code    34  hal_timer.o(i.hal_timer_init)
    hal_timer_start                          0x00019819   Thumb Code    78  hal_timer.o(i.hal_timer_start)
    hal_timer_stop                           0x0001986d   Thumb Code    40  hal_timer.o(i.hal_timer_stop)
    hal_uart_init                            0x00019895   Thumb Code   126  hal_uart.o(i.hal_uart_init)
    hal_uart_transmit_blocking               0x00019921   Thumb Code    12  hal_uart.o(i.hal_uart_transmit_blocking)
    handle_init                              0x00019931   Thumb Code   140  irq_redirect .o(i.handle_init)
    main                                     0x00019bad   Thumb Code    10  main.o(i.main)
    panel_init_code                          0x0001aa70   Data       12976  ap_demo.o(.constdata)
    phone_data_21                            0x0001dda0   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_55                            0x0001dda1   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_85_1                          0x0001dda2   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_92_1                          0x0001dda3   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_F5_1                          0x0001dda4   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_F5_2                          0x0001dda5   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_F5_3                          0x0001dda6   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_F5_4                          0x0001dda7   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_30                            0x0001dda8   Data           2  app_tp_for_custom_s8.o(.constdata)
    phone_data_52                            0x0001ddaa   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_data_92_3                          0x0001ddad   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_data_A3                            0x0001ddb0   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_data_A4                            0x0001ddb4   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_data_A5                            0x0001ddb8   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_data_AF                            0x0001ddbc   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_data_F1                            0x0001ddc0   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_data_22                            0x0001ddc4   Data           5  app_tp_for_custom_s8.o(.constdata)
    phone_data_92_2                          0x0001ddc9   Data           6  app_tp_for_custom_s8.o(.constdata)
    phone_data_F6_1                          0x0001ddcf   Data           6  app_tp_for_custom_s8.o(.constdata)
    phone_data_F6_2                          0x0001ddd5   Data           6  app_tp_for_custom_s8.o(.constdata)
    phone_data_F6_3                          0x0001dddb   Data           6  app_tp_for_custom_s8.o(.constdata)
    phone_data_F6_4                          0x0001dde1   Data           6  app_tp_for_custom_s8.o(.constdata)
    phone_data_60_1                          0x0001dde7   Data          16  app_tp_for_custom_s8.o(.constdata)
    phone_data_23                            0x0001ddf7   Data          11  app_tp_for_custom_s8.o(.constdata)
    phone_data_85_2                          0x0001de02   Data          28  app_tp_for_custom_s8.o(.constdata)
    phone_data_90                            0x0001de1e   Data          10  app_tp_for_custom_s8.o(.constdata)
    phone_data_72_0                          0x0001de28   Data          30  app_tp_for_custom_s8.o(.constdata)
    phone_data_72_1                          0x0001de46   Data          30  app_tp_for_custom_s8.o(.constdata)
    phone_data_72_2                          0x0001de64   Data         180  app_tp_for_custom_s8.o(.constdata)
    phone_data_72_3                          0x0001df18   Data          30  app_tp_for_custom_s8.o(.constdata)
    phone_data_80                            0x0001df36   Data         180  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_1                          0x0001dfea   Data         584  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_2                          0x0001e232   Data         584  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_5                          0x0001e47a   Data         584  app_tp_for_custom_s8.o(.constdata)
    sleep_on                                 0x0001e6c2   Data          16  app_tp_for_custom_s8.o(.constdata)
    screen_reg_start_data_size               0x0001e6d2   Data           1  app_tp_for_custom_s8.o(.constdata)
    Region$$Table$$Base                      0x0001eb88   Number         0  anon$$obj.o(Region$$Table)
    Region$$Table$$Limit                     0x0001ebb8   Number         0  anon$$obj.o(Region$$Table)
    g_fun_handle                             0x00070100   Data         192  irq_redirect .o(.ARM.__AT_0x00070100)
    phone_start_flag                         0x000701d5   Data           1  ap_demo.o(.data)
    phone_DisplayOFF_flag                    0x000701d6   Data           1  ap_demo.o(.data)
    panel_mode                               0x000701d7   Data           1  ap_demo.o(.data)
    phone_DisplayOFF_count                   0x000701de   Data           2  ap_demo.o(.data)
    value_reg_b1                             0x000701e4   Data           2  ap_demo.o(.data)
    value_reg_ca                             0x000701e6   Data           2  ap_demo.o(.data)
    value_reg_b1_bak                         0x000701e8   Data           2  ap_demo.o(.data)
    panel_r                                  0x000701ea   Data           2  ap_demo.o(.data)
    panel_g                                  0x000701ec   Data           2  ap_demo.o(.data)
    panel_b                                  0x000701ee   Data           2  ap_demo.o(.data)
    phone_data_E4                            0x00070200   Data           1  app_tp_for_custom_s8.o(.data)
    tp_flag                                  0x00070201   Data           1  app_tp_for_custom_s8.o(.data)
    g_phone_output_int_pad                   0x00070202   Data           1  app_tp_for_custom_s8.o(.data)
    tp_sleep_in                              0x00070203   Data           1  app_tp_for_custom_s8.o(.data)
    tp_sleep_count                           0x00070204   Data           1  app_tp_for_custom_s8.o(.data)
    sleep_double_EN                          0x00070205   Data           1  app_tp_for_custom_s8.o(.data)
    Flag_EA_EN                               0x00070206   Data           1  app_tp_for_custom_s8.o(.data)
    Flag_touch_count                         0x00070207   Data           1  app_tp_for_custom_s8.o(.data)
    touchnum_bak                             0x00070208   Data           1  app_tp_for_custom_s8.o(.data)
    Flag_blacklight_EN                       0x00070209   Data           1  app_tp_for_custom_s8.o(.data)
    phone_data_B1                            0x00070212   Data           2  app_tp_for_custom_s8.o(.data)
    phone_reg_coord_back                     0x0007021c   Data         200  app_tp_for_custom_s8.o(.data)
    g_screen_input_rst_pad                   0x000702e4   Data           1  app_tp_for_custom_s8.o(.data)
    g_screen_input_int_pad                   0x000702e5   Data           1  app_tp_for_custom_s8.o(.data)
    screen_data_write_1                      0x000702e6   Data           1  app_tp_for_custom_s8.o(.data)
    screen_data_write_2                      0x000702e7   Data           3  app_tp_for_custom_s8.o(.data)
    screen_data_write_3                      0x000702ea   Data           5  app_tp_for_custom_s8.o(.data)
    screen_reg_int_data                      0x000702f0   Data          48  app_tp_for_custom_s8.o(.data)
    s_screen_init_complate                   0x00070324   Data           1  app_tp_transfer.o(.data)
    u16TouchID                               0x00070328   Data           2  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data1               0x0007032a   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data3               0x0007032d   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data4               0x00070330   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_TP_Tuning_data2                 0x00070333   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_TP_Tuning_data3                 0x00070336   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_TP_Tuning_data6                 0x00070339   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_TP_Tuning_data7                 0x0007033c   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_TP_Tuning_data8                 0x0007033f   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_TP_Tuning_data4                 0x00070342   Data           4  app_tp_transfer.o(.data)
    MI10_PRO_TP_Tuning_data5                 0x00070346   Data           4  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data2               0x0007034a   Data           6  app_tp_transfer.o(.data)
    g_fls_w_cmd                              0x0007037c   Data           1  norflash.o(.data)
    g_fls_r_cmd                              0x0007037d   Data           1  norflash.o(.data)
    g_fls_write_en_status                    0x0007037e   Data           1  norflash.o(.data)
    isFlsTransferEnd                         0x0007037f   Data           1  norflash.o(.data)
    isFlsFifoReq                             0x00070380   Data           1  norflash.o(.data)
    isNandWriteCompleted                     0x00070381   Data           1  norflash.o(.data)
    isNandReadCompleted                      0x00070382   Data           1  norflash.o(.data)
    g_fls_error_info                         0x00070388   Data           6  norflash.o(.data)
    g_systick_cb_func                        0x00070394   Data           4  drv_common.o(.data)
    g_system_clock                           0x00070398   Data           4  drv_common.o(.data)
    g_scld_fhd_filter_h                      0x000703a8   Data         256  drv_param_init.o(.data)
    g_scld_fhd_filter_v                      0x000704a8   Data         256  drv_param_init.o(.data)
    g_scld_hd_filter_h                       0x000705a8   Data         256  drv_param_init.o(.data)
    g_scld_hd_filter_v                       0x000706a8   Data         256  drv_param_init.o(.data)
    g_sclu_filter                            0x000707a8   Data         128  drv_param_init.o(.data)
    g_ccm_setting                            0x00070828   Data          36  drv_param_init.o(.data)
    g_int_rxbr_irq0_cb_func                  0x00070858   Data           4  drv_rxbr.o(.data)
    g_int_rxbr_irq1_cb_func                  0x0007085c   Data           4  drv_rxbr.o(.data)
    g_int_vidc_cb_func                       0x0007086c   Data           4  drv_vidc.o(.data)
    tx_byte_num                              0x00070878   Data           4  drv_i2c_slave.o(.data)
    __stdout                                 0x0007089c   Data           4  stdout.o(.data)
    string                                   0x00070b38   Data         256  tau_log.o(.bss)
    hal_dmahandle                            0x00070c38   Data         160  hal_uart.o(.bss)
    hal_uarthandle_dma                       0x00070cd8   Data          32  hal_uart.o(.bss)
    hal_uart_handle_global                   0x00070cf8   Data          16  hal_uart.o(.bss)
    g_vsync_hande                            0x00070d08   Data          56  hal_internal_vsync.o(.bss)
    g_dcs_execute_table                      0x00070d40   Data        2048  hal_internal_vsync.o(.bss)
    g_packet_fifo                            0x00071660   Data        4144  dcs_packet_fifo.o(.bss)
    g_spis_ctrl_handle                       0x0007284c   Data          32  hal_spi_slave.o(.bss)
    __stack_limit                            0x00072870   Data           0  startup_armcm0.o(STACK)
    __initial_sp                             0x00073870   Data           0  startup_armcm0.o(STACK)



==============================================================================

Memory Map of the image

  Image Entry point : 0x000100c1

  Load Region LR_IROM2 (Base: 0x00010000, Size: 0x0000f288, Max: 0x00010000, ABSOLUTE, COMPRESSED[0x0000ef80])

    Execution Region ER_IROM2 (Exec base: 0x00010000, Load base: 0x00010000, Size: 0x0000ebb8, Max: 0x00010000, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00010000   0x00010000   0x000000c0   Data   RO          522    RESET               startup_armcm0.o
    0x000100c0   0x000100c0   0x00000000   Code   RO         2523  * .ARM.Collect$$$$00000000  mc_p.l(entry.o)
    0x000100c0   0x000100c0   0x00000004   Code   RO         2831    .ARM.Collect$$$$00000001  mc_p.l(entry2.o)
    0x000100c4   0x000100c4   0x00000004   Code   RO         2834    .ARM.Collect$$$$00000004  mc_p.l(entry5.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         2836    .ARM.Collect$$$$00000008  mc_p.l(entry7b.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         2838    .ARM.Collect$$$$0000000A  mc_p.l(entry8b.o)
    0x000100c8   0x000100c8   0x00000008   Code   RO         2839    .ARM.Collect$$$$0000000B  mc_p.l(entry9a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         2841    .ARM.Collect$$$$0000000D  mc_p.l(entry10a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         2843    .ARM.Collect$$$$0000000F  mc_p.l(entry11a.o)
    0x000100d0   0x000100d0   0x00000004   Code   RO         2832    .ARM.Collect$$$$00002712  mc_p.l(entry2.o)
    0x000100d4   0x000100d4   0x00000078   Code   RO          523    .text               startup_armcm0.o
    0x0001014c   0x0001014c   0x0000002c   Code   RO         2526    .text               mc_p.l(uidiv.o)
    0x00010178   0x00010178   0x00000028   Code   RO         2528    .text               mc_p.l(idiv.o)
    0x000101a0   0x000101a0   0x00000024   Code   RO         2530    .text               mc_p.l(memcpya.o)
    0x000101c4   0x000101c4   0x00000024   Code   RO         2532    .text               mc_p.l(memseta.o)
    0x000101e8   0x000101e8   0x000000b2   Code   RO         2797    .text               mf_p.l(fadd.o)
    0x0001029a   0x0001029a   0x0000007a   Code   RO         2799    .text               mf_p.l(fmul.o)
    0x00010314   0x00010314   0x0000007c   Code   RO         2801    .text               mf_p.l(fdiv.o)
    0x00010390   0x00010390   0x00000018   Code   RO         2803    .text               mf_p.l(fscalb.o)
    0x000103a8   0x000103a8   0x00000164   Code   RO         2805    .text               mf_p.l(dadd.o)
    0x0001050c   0x0001050c   0x000000d0   Code   RO         2807    .text               mf_p.l(dmul.o)
    0x000105dc   0x000105dc   0x000000f0   Code   RO         2809    .text               mf_p.l(ddiv.o)
    0x000106cc   0x000106cc   0x00000016   Code   RO         2811    .text               mf_p.l(fflti.o)
    0x000106e2   0x000106e2   0x0000000e   Code   RO         2813    .text               mf_p.l(ffltui.o)
    0x000106f0   0x000106f0   0x0000001c   Code   RO         2817    .text               mf_p.l(dfltui.o)
    0x0001070c   0x0001070c   0x00000032   Code   RO         2819    .text               mf_p.l(ffixi.o)
    0x0001073e   0x0001073e   0x00000028   Code   RO         2821    .text               mf_p.l(ffixui.o)
    0x00010766   0x00010766   0x00000002   PAD
    0x00010768   0x00010768   0x00000048   Code   RO         2823    .text               mf_p.l(dfixi.o)
    0x000107b0   0x000107b0   0x0000003c   Code   RO         2825    .text               mf_p.l(dfixui.o)
    0x000107ec   0x000107ec   0x00000028   Code   RO         2827    .text               mf_p.l(f2d.o)
    0x00010814   0x00010814   0x00000014   Code   RO         2829    .text               mf_p.l(cfrcmple.o)
    0x00010828   0x00010828   0x00000060   Code   RO         2846    .text               mc_p.l(uldiv.o)
    0x00010888   0x00010888   0x00000020   Code   RO         2848    .text               mc_p.l(llshl.o)
    0x000108a8   0x000108a8   0x00000022   Code   RO         2850    .text               mc_p.l(llushr.o)
    0x000108ca   0x000108ca   0x00000026   Code   RO         2852    .text               mc_p.l(llsshr.o)
    0x000108f0   0x000108f0   0x00000000   Code   RO         2854    .text               mc_p.l(iusefp.o)
    0x000108f0   0x000108f0   0x00000082   Code   RO         2855    .text               mf_p.l(fepilogue.o)
    0x00010972   0x00010972   0x000000be   Code   RO         2857    .text               mf_p.l(depilogue.o)
    0x00010a30   0x00010a30   0x00000040   Code   RO         2861    .text               mf_p.l(dfixul.o)
    0x00010a70   0x00010a70   0x00000028   Code   RO         2863    .text               mf_p.l(cdrcmple.o)
    0x00010a98   0x00010a98   0x00000024   Code   RO         2865    .text               mc_p.l(init.o)
    0x00010abc   0x00010abc   0x00000056   Code   RO         2875    .text               mc_p.l(__dczerorl2.o)
    0x00010b12   0x00010b12   0x00000002   PAD
    0x00010b14   0x00010b14   0x00000018   Code   RO         2072    i.ADC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010b2c   0x00010b2c   0x00000018   Code   RO         2073    i.AP_NRESET_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010b44   0x00010b44   0x00000014   Code   RO         2074    i.DMA_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010b58   0x00010b58   0x0000001c   Code   RO         2075    i.EXTI_INT0_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010b74   0x00010b74   0x0000001c   Code   RO         2076    i.EXTI_INT1_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010b90   0x00010b90   0x0000001c   Code   RO         2077    i.EXTI_INT2_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010bac   0x00010bac   0x0000001c   Code   RO         2078    i.EXTI_INT3_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010bc8   0x00010bc8   0x0000001c   Code   RO         2079    i.EXTI_INT4_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010be4   0x00010be4   0x0000001c   Code   RO         2080    i.EXTI_INT5_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c00   0x00010c00   0x0000001c   Code   RO         2081    i.EXTI_INT6_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c1c   0x00010c1c   0x0000001c   Code   RO         2082    i.EXTI_INT7_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c38   0x00010c38   0x00000014   Code   RO         2083    i.FLSCTRL_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c4c   0x00010c4c   0x0000004e   Code   RO           99    i.Gpio_swire_output  ap_demo.o
    0x00010c9a   0x00010c9a   0x00000002   PAD
    0x00010c9c   0x00010c9c   0x00000014   Code   RO         2084    i.HardFault_Handler  CVWL568.lib(irq_redirect .o)
    0x00010cb0   0x00010cb0   0x00000018   Code   RO         2085    i.I2C0_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010cc8   0x00010cc8   0x00000018   Code   RO         2086    i.I2C1_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010ce0   0x00010ce0   0x00000018   Code   RO         2087    i.LCDC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010cf8   0x00010cf8   0x00000028   Code   RO          939    i.LOG_printf        CVWL568.lib(tau_log.o)
    0x00010d20   0x00010d20   0x00000018   Code   RO         2088    i.MEMC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010d38   0x00010d38   0x00000018   Code   RO         2089    i.MIPI_RX_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010d50   0x00010d50   0x00000018   Code   RO         2090    i.MIPI_TX_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010d68   0x00010d68   0x0000001c   Code   RO         2091    i.PWMDET_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010d84   0x00010d84   0x000000b0   Code   RO          101    i.PWM_Task          ap_demo.o
    0x00010e34   0x00010e34   0x00000134   Code   RO          357    i.S20_Start_init    app_tp_transfer.o
    0x00010f68   0x00010f68   0x0000001c   Code   RO         2092    i.SPIM_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010f84   0x00010f84   0x0000001c   Code   RO         2093    i.SPIS_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010fa0   0x00010fa0   0x0000001c   Code   RO         2094    i.SWIRE_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010fbc   0x00010fbc   0x00000018   Code   RO         2095    i.SysTick_Handler   CVWL568.lib(irq_redirect .o)
    0x00010fd4   0x00010fd4   0x00000018   Code   RO         2096    i.TIMER0_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010fec   0x00010fec   0x00000002   Code   RO         2367    i.UART_DisableDma   CVWL568.lib(drv_uart.o)
    0x00010fee   0x00010fee   0x00000004   Code   RO         2373    i.UART_GetInstance  CVWL568.lib(drv_uart.o)
    0x00010ff2   0x00010ff2   0x0000000e   Code   RO         2869    i.__scatterload_copy  mc_p.l(handlers.o)
    0x00011000   0x00011000   0x00000014   Data   RO         1147    .ARM.__at_0x11000   CVWL568.lib(drv_common.o)
    0x00011014   0x00011014   0x00000018   Code   RO         2097    i.TIMER1_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x0001102c   0x0001102c   0x00000018   Code   RO         2098    i.TIMER2_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00011044   0x00011044   0x00000018   Code   RO         2099    i.TIMER3_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x0001105c   0x0001105c   0x0000001c   Code   RO         2363    i.UART0_IRQ_Handle  CVWL568.lib(drv_uart.o)
    0x00011078   0x00011078   0x00000018   Code   RO         2100    i.UART_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00011090   0x00011090   0x00000024   Code   RO         2381    i.UART_ResetRxFIFO  CVWL568.lib(drv_uart.o)
    0x000110b4   0x000110b4   0x00000048   Code   RO         2384    i.UART_SetBaudRate  CVWL568.lib(drv_uart.o)
    0x000110fc   0x000110fc   0x0000001a   Code   RO         2385    i.UART_SwitchSCLK   CVWL568.lib(drv_uart.o)
    0x00011116   0x00011116   0x00000134   Code   RO         2387    i.UART_TransferHandleIRQ  CVWL568.lib(drv_uart.o)
    0x0001124a   0x0001124a   0x0000001a   Code   RO         2389    i.UART_WriteBlocking  CVWL568.lib(drv_uart.o)
    0x00011264   0x00011264   0x000000bc   Code   RO         2390    i.UART_init         CVWL568.lib(drv_uart.o)
    0x00011320   0x00011320   0x00000018   Code   RO         2101    i.VIDC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00011338   0x00011338   0x00000018   Code   RO         2102    i.VPRE_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00011350   0x00011350   0x00000018   Code   RO         2103    i.WDG_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00011368   0x00011368   0x00000020   Code   RO         2769    i.__0printf         mc_p.l(printfa.o)
    0x00011388   0x00011388   0x00000024   Code   RO         2775    i.__0vsprintf       mc_p.l(printfa.o)
    0x000113ac   0x000113ac   0x0000002e   Code   RO         2859    i.__ARM_clz         mf_p.l(depilogue.o)
    0x000113da   0x000113da   0x0000001a   Code   RO          610    i.__ARM_common_switch8  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000113f4   0x000113f4   0x00000018   Code   RO         2165    i.__NVIC_ClearPendingIRQ  CVWL568.lib(drv_i2c_master.o)
    0x0001140c   0x0001140c   0x00000018   Code   RO         2198    i.__NVIC_ClearPendingIRQ  CVWL568.lib(drv_i2c_slave.o)
    0x00011424   0x00011424   0x00000018   Code   RO         2233    i.__NVIC_ClearPendingIRQ  CVWL568.lib(drv_spi_master.o)
    0x0001143c   0x0001143c   0x00000020   Code   RO         1812    i.__NVIC_DisableIRQ  CVWL568.lib(drv_rxbr.o)
    0x0001145c   0x0001145c   0x00000018   Code   RO         1813    i.__NVIC_EnableIRQ  CVWL568.lib(drv_rxbr.o)
    0x00011474   0x00011474   0x00000044   Code   RO         2295    i.__NVIC_SetPriority  CVWL568.lib(hal_spi_slave.o)
    0x000114b8   0x000114b8   0x00000002   Code   RO         2870    i.__scatterload_null  mc_p.l(handlers.o)
    0x000114ba   0x000114ba   0x0000000e   Code   RO         2871    i.__scatterload_zeroinit  mc_p.l(handlers.o)
    0x000114c8   0x000114c8   0x00000174   Code   RO         2776    i._fp_digits        mc_p.l(printfa.o)
    0x0001163c   0x0001163c   0x000006ec   Code   RO         2777    i._printf_core      mc_p.l(printfa.o)
    0x00011d28   0x00011d28   0x00000020   Code   RO         2778    i._printf_post_padding  mc_p.l(printfa.o)
    0x00011d48   0x00011d48   0x0000002c   Code   RO         2779    i._printf_pre_padding  mc_p.l(printfa.o)
    0x00011d74   0x00011d74   0x0000000a   Code   RO         2781    i._sputc            mc_p.l(printfa.o)
    0x00011d7e   0x00011d7e   0x00000002   PAD
    0x00011d80   0x00011d80   0x00001184   Code   RO          102    i.ap_dcs_read       ap_demo.o
    0x00012f04   0x00012f04   0x000001ac   Code   RO          103    i.ap_demo           ap_demo.o
    0x000130b0   0x000130b0   0x00000018   Code   RO          104    i.ap_get_reg_ca     ap_demo.o
    0x000130c8   0x000130c8   0x0000008c   Code   RO          105    i.ap_get_reg_df     ap_demo.o
    0x00013154   0x00013154   0x00000064   Code   RO          106    i.ap_reset_cb       ap_demo.o
    0x000131b8   0x000131b8   0x000000e0   Code   RO          107    i.ap_set_backlight  ap_demo.o
    0x00013298   0x00013298   0x00000058   Code   RO          108    i.ap_set_display_off  ap_demo.o
    0x000132f0   0x000132f0   0x00000038   Code   RO          109    i.ap_set_display_on  ap_demo.o
    0x00013328   0x00013328   0x00000088   Code   RO          110    i.ap_set_enter_sleep_mode  ap_demo.o
    0x000133b0   0x000133b0   0x00000048   Code   RO          111    i.ap_set_exit_sleep_mode  ap_demo.o
    0x000133f8   0x000133f8   0x0000001c   Code   RO          112    i.ap_set_tp_calibration_04  ap_demo.o
    0x00013414   0x00013414   0x000000b0   Code   RO          358    i.ap_tp_calibration  app_tp_transfer.o
    0x000134c4   0x000134c4   0x0000001c   Code   RO         1814    i.app_ADC_IRQn_Handler  CVWL568.lib(drv_rxbr.o)
    0x000134e0   0x000134e0   0x00000024   Code   RO         1563    i.app_AP_NRESET_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00013504   0x00013504   0x0000001c   Code   RO         1564    i.app_EXTI_INT0_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00013520   0x00013520   0x0000001c   Code   RO         1565    i.app_EXTI_INT1_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x0001353c   0x0001353c   0x0000001c   Code   RO         1566    i.app_EXTI_INT2_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00013558   0x00013558   0x0000001c   Code   RO         1567    i.app_EXTI_INT3_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00013574   0x00013574   0x0000001c   Code   RO         1568    i.app_EXTI_INT4_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00013590   0x00013590   0x0000001c   Code   RO         1569    i.app_EXTI_INT5_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x000135ac   0x000135ac   0x0000001c   Code   RO         1570    i.app_EXTI_INT6_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x000135c8   0x000135c8   0x0000001c   Code   RO         1571    i.app_EXTI_INT7_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x000135e4   0x000135e4   0x00000048   Code   RO         1139    i.app_HardFault_Handler  CVWL568.lib(drv_common.o)
    0x0001362c   0x0001362c   0x00000010   Code   RO         2199    i.app_I2C0_IRQn_Handler  CVWL568.lib(drv_i2c_slave.o)
    0x0001363c   0x0001363c   0x00000010   Code   RO         2166    i.app_I2C1_IRQn_Handler  CVWL568.lib(drv_i2c_master.o)
    0x0001364c   0x0001364c   0x000000e0   Code   RO          969    i.app_LCDC_IRQn_Handler  CVWL568.lib(hal_internal_vsync.o)
    0x0001372c   0x0001372c   0x00000088   Code   RO         1697    i.app_MEMC_IRQn_Handler  CVWL568.lib(drv_memc.o)
    0x000137b4   0x000137b4   0x0000028c   Code   RO         1304    i.app_MIPI_RX_IRQn_Handler  CVWL568.lib(drv_dsi_rx.o)
    0x00013a40   0x00013a40   0x000000a0   Code   RO         1360    i.app_MIPI_TX_IRQn_Handler  CVWL568.lib(drv_dsi_tx.o)
    0x00013ae0   0x00013ae0   0x00000048   Code   RO         1773    i.app_PWMDET_IRQn_Handler  CVWL568.lib(drv_pwm.o)
    0x00013b28   0x00013b28   0x00000030   Code   RO         2234    i.app_SPIM_IRQn_Handler  CVWL568.lib(drv_spi_master.o)
    0x00013b58   0x00013b58   0x000000a4   Code   RO         2296    i.app_SPIS_IRQn_Handler  CVWL568.lib(hal_spi_slave.o)
    0x00013bfc   0x00013bfc   0x00000020   Code   RO         1905    i.app_SWIRE_IRQn_Handler  CVWL568.lib(drv_swire.o)
    0x00013c1c   0x00013c1c   0x00000018   Code   RO         1140    i.app_SysTick_Handler  CVWL568.lib(drv_common.o)
    0x00013c34   0x00013c34   0x00000024   Code   RO         1955    i.app_TIMER0_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x00013c58   0x00013c58   0x00000024   Code   RO         1956    i.app_TIMER1_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x00013c7c   0x00013c7c   0x00000024   Code   RO         1957    i.app_TIMER2_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x00013ca0   0x00013ca0   0x00000034   Code   RO         1958    i.app_TIMER3_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x00013cd4   0x00013cd4   0x00000008   Code   RO         2391    i.app_UART_IRQn_Handler  CVWL568.lib(drv_uart.o)
    0x00013cdc   0x00013cdc   0x0000001c   Code   RO         1993    i.app_VIDC_IRQn_Handler  CVWL568.lib(drv_vidc.o)
    0x00013cf8   0x00013cf8   0x0000001c   Code   RO         1815    i.app_VPRE_IRQn_Handler  CVWL568.lib(drv_rxbr.o)
    0x00013d14   0x00013d14   0x0000002c   Code   RO         2450    i.app_WDG_IRQn_Handler  CVWL568.lib(drv_wdg.o)
    0x00013d40   0x00013d40   0x00000010   Code   RO         1251    i.app_dma_irq_handler  CVWL568.lib(drv_dma.o)
    0x00013d50   0x00013d50   0x00000030   Code   RO         1044    i.app_fls_ctrl_Handler  CVWL568.lib(norflash.o)
    0x00013d80   0x00013d80   0x00000024   Code   RO          359    i.app_tp_I2C_init   app_tp_transfer.o
    0x00013da4   0x00013da4   0x0000005c   Code   RO          113    i.app_tp_calibration_exec  ap_demo.o
    0x00013e00   0x00013e00   0x00000030   Code   RO          360    i.app_tp_i2cs_callback  app_tp_transfer.o
    0x00013e30   0x00013e30   0x00000048   Code   RO          361    i.app_tp_init       app_tp_transfer.o
    0x00013e78   0x00013e78   0x00000020   Code   RO          362    i.app_tp_m_read     app_tp_transfer.o
    0x00013e98   0x00013e98   0x00000008   Code   RO          364    i.app_tp_m_write    app_tp_transfer.o
    0x00013ea0   0x00013ea0   0x00000318   Code   RO          265    i.app_tp_phone_analysis_data  app_tp_for_custom_s8.o
    0x000141b8   0x000141b8   0x0000000c   Code   RO          365    i.app_tp_phone_clear_reset_on  app_tp_transfer.o
    0x000141c4   0x000141c4   0x00000008   Code   RO          367    i.app_tp_s_read     app_tp_transfer.o
    0x000141cc   0x000141cc   0x00000008   Code   RO          369    i.app_tp_s_write    app_tp_transfer.o
    0x000141d4   0x000141d4   0x0000029c   Code   RO          267    i.app_tp_screen_analysis_int  app_tp_for_custom_s8.o
    0x00014470   0x00014470   0x00000030   Code   RO          370    i.app_tp_screen_init  app_tp_transfer.o
    0x000144a0   0x000144a0   0x0000000c   Code   RO          371    i.app_tp_screen_int_callback  app_tp_transfer.o
    0x000144ac   0x000144ac   0x00000040   Code   RO          372    i.app_tp_transfer_screen_const  app_tp_transfer.o
    0x000144ec   0x000144ec   0x000000ec   Code   RO          373    i.app_tp_transfer_screen_int  app_tp_transfer.o
    0x000145d8   0x000145d8   0x00000018   Code   RO          374    i.app_tp_transfer_screen_start  app_tp_transfer.o
    0x000145f0   0x000145f0   0x0000001c   Code   RO          502    i.board_Init        board.o
    0x0001460c   0x0001460c   0x000002b4   Code   RO          970    i.calc_framebuffer_setting  CVWL568.lib(hal_internal_vsync.o)
    0x000148c0   0x000148c0   0x000000c8   Code   RO         2520    i.ceil              m_ps.l(ceil.o)
    0x00014988   0x00014988   0x0000002c   Code   RO          971    i.check_mipi_rx_tx_video_info  CVWL568.lib(hal_internal_vsync.o)
    0x000149b4   0x000149b4   0x00000090   Code   RO          972    i.check_pkt_buf_rev  CVWL568.lib(hal_internal_vsync.o)
    0x00014a44   0x00014a44   0x00000058   Code   RO         1126    i.dcs_packet_fifo_alloc  CVWL568.lib(dcs_packet_fifo.o)
    0x00014a9c   0x00014a9c   0x00000018   Code   RO         1127    i.dcs_packet_fifo_init  CVWL568.lib(dcs_packet_fifo.o)
    0x00014ab4   0x00014ab4   0x00000044   Code   RO         1128    i.dcs_packet_free_fifo_header  CVWL568.lib(dcs_packet_fifo.o)
    0x00014af8   0x00014af8   0x00000024   Code   RO         1129    i.dcs_packet_get_fifo_header  CVWL568.lib(dcs_packet_fifo.o)
    0x00014b1c   0x00014b1c   0x0000001c   Code   RO          973    i.dcs_sw_filter     CVWL568.lib(hal_internal_vsync.o)
    0x00014b38   0x00014b38   0x00000018   Code   RO          931    i.delayMs           CVWL568.lib(tau_delay.o)
    0x00014b50   0x00014b50   0x00000022   Code   RO          932    i.delayUs           CVWL568.lib(tau_delay.o)
    0x00014b72   0x00014b72   0x00000002   PAD
    0x00014b74   0x00014b74   0x00000038   Code   RO         1924    i.drv_ap_rst_trig_edge_detect  CVWL568.lib(drv_sys_cfg.o)
    0x00014bac   0x00014bac   0x0000000c   Code   RO         2266    i.drv_chip_info_get_info  CVWL568.lib(drv_chip_info.o)
    0x00014bb8   0x00014bb8   0x00000040   Code   RO         2267    i.drv_chip_info_init  CVWL568.lib(drv_chip_info.o)
    0x00014bf8   0x00014bf8   0x000000c8   Code   RO         2268    i.drv_chip_rx_info_check  CVWL568.lib(drv_chip_info.o)
    0x00014cc0   0x00014cc0   0x00000014   Code   RO         2269    i.drv_chip_rx_init_done  CVWL568.lib(drv_chip_info.o)
    0x00014cd4   0x00014cd4   0x00000058   Code   RO         1142    i.drv_common_enable_systick  CVWL568.lib(drv_common.o)
    0x00014d2c   0x00014d2c   0x00000008   Code   RO         1145    i.drv_common_system_init  CVWL568.lib(drv_common.o)
    0x00014d34   0x00014d34   0x0000000c   Code   RO         1161    i.drv_crgu_clear_all_reset_flags  CVWL568.lib(drv_crgu.o)
    0x00014d40   0x00014d40   0x00000010   Code   RO         1166    i.drv_crgu_config_reset_modules  CVWL568.lib(drv_crgu.o)
    0x00014d50   0x00014d50   0x00000014   Code   RO         1178    i.drv_crgu_set_ahb_pre_div  CVWL568.lib(drv_crgu.o)
    0x00014d64   0x00014d64   0x00000014   Code   RO         1179    i.drv_crgu_set_ahb_src  CVWL568.lib(drv_crgu.o)
    0x00014d78   0x00014d78   0x00000020   Code   RO         1182    i.drv_crgu_set_clock  CVWL568.lib(drv_crgu.o)
    0x00014d98   0x00014d98   0x00000014   Code   RO         1183    i.drv_crgu_set_dpi_mux_src  CVWL568.lib(drv_crgu.o)
    0x00014dac   0x00014dac   0x00000018   Code   RO         1184    i.drv_crgu_set_dpi_pre_div  CVWL568.lib(drv_crgu.o)
    0x00014dc4   0x00014dc4   0x00000014   Code   RO         1185    i.drv_crgu_set_dpi_pre_src  CVWL568.lib(drv_crgu.o)
    0x00014dd8   0x00014dd8   0x00000014   Code   RO         1186    i.drv_crgu_set_dsc_core_div  CVWL568.lib(drv_crgu.o)
    0x00014dec   0x00014dec   0x00000014   Code   RO         1187    i.drv_crgu_set_dsco_src  CVWL568.lib(drv_crgu.o)
    0x00014e00   0x00014e00   0x00000014   Code   RO         1188    i.drv_crgu_set_dsco_src_div  CVWL568.lib(drv_crgu.o)
    0x00014e14   0x00014e14   0x00000014   Code   RO         1189    i.drv_crgu_set_fb_div  CVWL568.lib(drv_crgu.o)
    0x00014e28   0x00014e28   0x00000014   Code   RO         1190    i.drv_crgu_set_fb_src  CVWL568.lib(drv_crgu.o)
    0x00014e3c   0x00014e3c   0x00000014   Code   RO         1193    i.drv_crgu_set_lcdc_div  CVWL568.lib(drv_crgu.o)
    0x00014e50   0x00014e50   0x00000014   Code   RO         1194    i.drv_crgu_set_lcdc_src  CVWL568.lib(drv_crgu.o)
    0x00014e64   0x00014e64   0x00000014   Code   RO         1195    i.drv_crgu_set_mipi_cfg_src  CVWL568.lib(drv_crgu.o)
    0x00014e78   0x00014e78   0x00000018   Code   RO         1196    i.drv_crgu_set_mipi_ref_src  CVWL568.lib(drv_crgu.o)
    0x00014e90   0x00014e90   0x00000018   Code   RO         1199    i.drv_crgu_set_reset  CVWL568.lib(drv_crgu.o)
    0x00014ea8   0x00014ea8   0x00000014   Code   RO         1200    i.drv_crgu_set_rxbr_div  CVWL568.lib(drv_crgu.o)
    0x00014ebc   0x00014ebc   0x00000014   Code   RO         1201    i.drv_crgu_set_rxbr_src  CVWL568.lib(drv_crgu.o)
    0x00014ed0   0x00014ed0   0x00000014   Code   RO         1203    i.drv_crgu_set_vidc_src  CVWL568.lib(drv_crgu.o)
    0x00014ee4   0x00014ee4   0x00000018   Code   RO         1255    i.drv_dma_clear_flag  CVWL568.lib(drv_dma.o)
    0x00014efc   0x00014efc   0x0000001c   Code   RO         1256    i.drv_dma_create_handle  CVWL568.lib(drv_dma.o)
    0x00014f18   0x00014f18   0x00000010   Code   RO         1258    i.drv_dma_disenable_channel  CVWL568.lib(drv_dma.o)
    0x00014f28   0x00014f28   0x00000010   Code   RO         1260    i.drv_dma_enable_channel  CVWL568.lib(drv_dma.o)
    0x00014f38   0x00014f38   0x00000024   Code   RO         1261    i.drv_dma_enable_channel_interrupts  CVWL568.lib(drv_dma.o)
    0x00014f5c   0x00014f5c   0x0000000c   Code   RO         1263    i.drv_dma_get_channel_flag  CVWL568.lib(drv_dma.o)
    0x00014f68   0x00014f68   0x00000090   Code   RO         1266    i.drv_dma_irq_handler  CVWL568.lib(drv_dma.o)
    0x00014ff8   0x00014ff8   0x00000012   Code   RO         1268    i.drv_dma_prepar_transfer  CVWL568.lib(drv_dma.o)
    0x0001500a   0x0001500a   0x0000001a   Code   RO         1270    i.drv_dma_set_burst  CVWL568.lib(drv_dma.o)
    0x00015024   0x00015024   0x00000006   Code   RO         1271    i.drv_dma_set_callback  CVWL568.lib(drv_dma.o)
    0x0001502a   0x0001502a   0x00000002   PAD
    0x0001502c   0x0001502c   0x00000044   Code   RO         1273    i.drv_dma_set_transfer  CVWL568.lib(drv_dma.o)
    0x00015070   0x00015070   0x00000036   Code   RO         2279    i.drv_dsc_dec_convert_pps_rc_parameter  CVWL568.lib(drv_dsc_dec.o)
    0x000150a6   0x000150a6   0x0000000c   Code   RO         2280    i.drv_dsc_dec_disable  CVWL568.lib(drv_dsc_dec.o)
    0x000150b2   0x000150b2   0x00000002   PAD
    0x000150b4   0x000150b4   0x00000074   Code   RO         2281    i.drv_dsc_dec_enable  CVWL568.lib(drv_dsc_dec.o)
    0x00015128   0x00015128   0x0000000a   Code   RO         2282    i.drv_dsc_dec_get_nslc  CVWL568.lib(drv_dsc_dec.o)
    0x00015132   0x00015132   0x00000028   Code   RO         2284    i.drv_dsc_dec_set_u8_pps  CVWL568.lib(drv_dsc_dec.o)
    0x0001515a   0x0001515a   0x00000002   PAD
    0x0001515c   0x0001515c   0x00000104   Code   RO         1305    i.drv_dsi_rx_calc_ipi_tx_delay  CVWL568.lib(drv_dsi_rx.o)
    0x00015260   0x00015260   0x00000040   Code   RO         1306    i.drv_dsi_rx_enable_irq  CVWL568.lib(drv_dsi_rx.o)
    0x000152a0   0x000152a0   0x00000050   Code   RO         1307    i.drv_dsi_rx_get_color_bpp  CVWL568.lib(drv_dsi_rx.o)
    0x000152f0   0x000152f0   0x0000001c   Code   RO         1308    i.drv_dsi_rx_get_color_pcc  CVWL568.lib(drv_dsi_rx.o)
    0x0001530c   0x0001530c   0x00000008   Code   RO         1309    i.drv_dsi_rx_get_compression_en  CVWL568.lib(drv_dsi_rx.o)
    0x00015314   0x00015314   0x00000006   Code   RO         1310    i.drv_dsi_rx_get_max_ret_size  CVWL568.lib(drv_dsi_rx.o)
    0x0001531a   0x0001531a   0x0000000e   Code   RO         1314    i.drv_dsi_rx_power_up  CVWL568.lib(drv_dsi_rx.o)
    0x00015328   0x00015328   0x00000020   Code   RO         1315    i.drv_dsi_rx_set_ctrl_cfg  CVWL568.lib(drv_dsi_rx.o)
    0x00015348   0x00015348   0x00000010   Code   RO         1316    i.drv_dsi_rx_set_ddi_cfg  CVWL568.lib(drv_dsi_rx.o)
    0x00015358   0x00015358   0x00000004   Code   RO         1318    i.drv_dsi_rx_set_inten  CVWL568.lib(drv_dsi_rx.o)
    0x0001535c   0x0001535c   0x00000010   Code   RO         1319    i.drv_dsi_rx_set_ipi_cfg  CVWL568.lib(drv_dsi_rx.o)
    0x0001536c   0x0001536c   0x00000046   Code   RO         1321    i.drv_dsi_rx_set_lane_swap  CVWL568.lib(drv_dsi_rx.o)
    0x000153b2   0x000153b2   0x00000002   PAD
    0x000153b4   0x000153b4   0x000000d0   Code   RO         1322    i.drv_dsi_rx_set_up_phy  CVWL568.lib(drv_dsi_rx.o)
    0x00015484   0x00015484   0x0000000e   Code   RO         1323    i.drv_dsi_rx_shut_down  CVWL568.lib(drv_dsi_rx.o)
    0x00015492   0x00015492   0x00000014   Code   RO         1362    i.drv_dsi_tx_command_header  CVWL568.lib(drv_dsi_tx.o)
    0x000154a6   0x000154a6   0x0000006c   Code   RO         1363    i.drv_dsi_tx_command_mode_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x00015512   0x00015512   0x00000004   Code   RO         1364    i.drv_dsi_tx_command_put_payload  CVWL568.lib(drv_dsi_tx.o)
    0x00015516   0x00015516   0x00000018   Code   RO         1365    i.drv_dsi_tx_config_eotp  CVWL568.lib(drv_dsi_tx.o)
    0x0001552e   0x0001552e   0x00000008   Code   RO         1366    i.drv_dsi_tx_config_int  CVWL568.lib(drv_dsi_tx.o)
    0x00015536   0x00015536   0x00000008   Code   RO         1367    i.drv_dsi_tx_dpi_lpcmd_time  CVWL568.lib(drv_dsi_tx.o)
    0x0001553e   0x0001553e   0x0000000a   Code   RO         1368    i.drv_dsi_tx_dpi_mode  CVWL568.lib(drv_dsi_tx.o)
    0x00015548   0x00015548   0x00000024   Code   RO         1369    i.drv_dsi_tx_dpi_polarity  CVWL568.lib(drv_dsi_tx.o)
    0x0001556c   0x0001556c   0x00000004   Code   RO         1370    i.drv_dsi_tx_edpi_cmd_size  CVWL568.lib(drv_dsi_tx.o)
    0x00015570   0x00015570   0x00000004   Code   RO         1372    i.drv_dsi_tx_get_cmd_status  CVWL568.lib(drv_dsi_tx.o)
    0x00015574   0x00015574   0x00000004   Code   RO         1374    i.drv_dsi_tx_mode   CVWL568.lib(drv_dsi_tx.o)
    0x00015578   0x00015578   0x00000018   Code   RO         1375    i.drv_dsi_tx_phy_clock_lane_auto_lp  CVWL568.lib(drv_dsi_tx.o)
    0x00015590   0x00015590   0x0000001a   Code   RO         1376    i.drv_dsi_tx_phy_clock_lane_req_hs  CVWL568.lib(drv_dsi_tx.o)
    0x000155aa   0x000155aa   0x0000000c   Code   RO         1378    i.drv_dsi_tx_phy_lane_mode  CVWL568.lib(drv_dsi_tx.o)
    0x000155b6   0x000155b6   0x00000064   Code   RO         1382    i.drv_dsi_tx_phy_status_ready  CVWL568.lib(drv_dsi_tx.o)
    0x0001561a   0x0001561a   0x0000003e   Code   RO         1383    i.drv_dsi_tx_phy_status_stopstate  CVWL568.lib(drv_dsi_tx.o)
    0x00015658   0x00015658   0x0000001e   Code   RO         1385    i.drv_dsi_tx_phy_time_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x00015676   0x00015676   0x00000008   Code   RO         1389    i.drv_dsi_tx_powerup  CVWL568.lib(drv_dsi_tx.o)
    0x0001567e   0x0001567e   0x0000001c   Code   RO         1390    i.drv_dsi_tx_response_mode  CVWL568.lib(drv_dsi_tx.o)
    0x0001569a   0x0001569a   0x00000018   Code   RO         1393    i.drv_dsi_tx_set_bta_ack  CVWL568.lib(drv_dsi_tx.o)
    0x000156b2   0x000156b2   0x0000000c   Code   RO         1394    i.drv_dsi_tx_set_esc_div  CVWL568.lib(drv_dsi_tx.o)
    0x000156be   0x000156be   0x00000002   PAD
    0x000156c0   0x000156c0   0x00000034   Code   RO         1395    i.drv_dsi_tx_set_int  CVWL568.lib(drv_dsi_tx.o)
    0x000156f4   0x000156f4   0x00000010   Code   RO         1396    i.drv_dsi_tx_set_time_out_div  CVWL568.lib(drv_dsi_tx.o)
    0x00015704   0x00015704   0x00000008   Code   RO         1397    i.drv_dsi_tx_set_video_chunk  CVWL568.lib(drv_dsi_tx.o)
    0x0001570c   0x0001570c   0x00000022   Code   RO         1398    i.drv_dsi_tx_set_video_timing  CVWL568.lib(drv_dsi_tx.o)
    0x0001572e   0x0001572e   0x00000008   Code   RO         1400    i.drv_dsi_tx_shutdown  CVWL568.lib(drv_dsi_tx.o)
    0x00015736   0x00015736   0x00000026   Code   RO         1401    i.drv_dsi_tx_timeout_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x0001575c   0x0001575c   0x000000aa   Code   RO         1404    i.drv_dsi_tx_video_mode_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x00015806   0x00015806   0x00000016   Code   RO         1405    i.drv_dsi_tx_video_mode_disable_hact_cmd  CVWL568.lib(drv_dsi_tx.o)
    0x0001581c   0x0001581c   0x00000018   Code   RO         1406    i.drv_dsi_tx_video_mode_set_lp_cmd  CVWL568.lib(drv_dsi_tx.o)
    0x00015834   0x00015834   0x00000020   Code   RO         2474    i.drv_efuse_enter_inactive  CVWL568.lib(drv_efuse.o)
    0x00015854   0x00015854   0x0000000c   Code   RO         2477    i.drv_efuse_int_enable  CVWL568.lib(drv_efuse.o)
    0x00015860   0x00015860   0x00000032   Code   RO         2478    i.drv_efuse_read    CVWL568.lib(drv_efuse.o)
    0x00015892   0x00015892   0x00000018   Code   RO         2479    i.drv_efuse_read_req  CVWL568.lib(drv_efuse.o)
    0x000158aa   0x000158aa   0x00000002   PAD
    0x000158ac   0x000158ac   0x00000018   Code   RO         1572    i.drv_gpio_get_input_data  CVWL568.lib(drv_gpio.o)
    0x000158c4   0x000158c4   0x0000000c   Code   RO         1574    i.drv_gpio_register_ap_reset_callback  CVWL568.lib(drv_gpio.o)
    0x000158d0   0x000158d0   0x00000014   Code   RO         1575    i.drv_gpio_register_callback  CVWL568.lib(drv_gpio.o)
    0x000158e4   0x000158e4   0x00000044   Code   RO         1577    i.drv_gpio_set_int  CVWL568.lib(drv_gpio.o)
    0x00015928   0x00015928   0x00000020   Code   RO         1578    i.drv_gpio_set_ioe  CVWL568.lib(drv_gpio.o)
    0x00015948   0x00015948   0x00000010   Code   RO         1579    i.drv_gpio_set_mode0  CVWL568.lib(drv_gpio.o)
    0x00015958   0x00015958   0x00000010   Code   RO         1580    i.drv_gpio_set_mode1  CVWL568.lib(drv_gpio.o)
    0x00015968   0x00015968   0x00000010   Code   RO         1581    i.drv_gpio_set_mode2  CVWL568.lib(drv_gpio.o)
    0x00015978   0x00015978   0x00000010   Code   RO         1582    i.drv_gpio_set_mode3  CVWL568.lib(drv_gpio.o)
    0x00015988   0x00015988   0x00000020   Code   RO          705    i.drv_gpio_set_output_data  CVWL568.lib(hal_gpio.o)
    0x000159a8   0x000159a8   0x00000130   Code   RO         1583    i.drv_gpio_set_pull_state  CVWL568.lib(drv_gpio.o)
    0x00015ad8   0x00015ad8   0x00000034   Code   RO         1615    i.drv_i2c_dma_callback  CVWL568.lib(drv_i2c_dma.o)
    0x00015b0c   0x00015b0c   0x000000ac   Code   RO         1616    i.drv_i2c_dma_init  CVWL568.lib(drv_i2c_dma.o)
    0x00015bb8   0x00015bb8   0x0000001a   Code   RO         1617    i.drv_i2c_enable_rx_dma  CVWL568.lib(drv_i2c_dma.o)
    0x00015bd2   0x00015bd2   0x00000018   Code   RO         1618    i.drv_i2c_enable_tx_dma  CVWL568.lib(drv_i2c_dma.o)
    0x00015bea   0x00015bea   0x00000002   PAD
    0x00015bec   0x00015bec   0x00000060   Code   RO         2168    i.drv_i2c_m_clear_it_pending_bit  CVWL568.lib(drv_i2c_master.o)
    0x00015c4c   0x00015c4c   0x00000010   Code   RO         2170    i.drv_i2c_m_enable  CVWL568.lib(drv_i2c_master.o)
    0x00015c5c   0x00015c5c   0x00000038   Code   RO         2171    i.drv_i2c_m_enable_intr  CVWL568.lib(drv_i2c_master.o)
    0x00015c94   0x00015c94   0x0000000c   Code   RO         2174    i.drv_i2c_m_set_callback  CVWL568.lib(drv_i2c_master.o)
    0x00015ca0   0x00015ca0   0x0000008c   Code   RO         2178    i.drv_i2c_master_init  CVWL568.lib(drv_i2c_master.o)
    0x00015d2c   0x00015d2c   0x0000005c   Code   RO         1619    i.drv_i2c_master_read_dma  CVWL568.lib(drv_i2c_dma.o)
    0x00015d88   0x00015d88   0x0000003c   Code   RO         1620    i.drv_i2c_master_write_dma  CVWL568.lib(drv_i2c_dma.o)
    0x00015dc4   0x00015dc4   0x0000002e   Code   RO         1621    i.drv_i2c_master_write_read_cmd  CVWL568.lib(drv_i2c_dma.o)
    0x00015df2   0x00015df2   0x00000002   PAD
    0x00015df4   0x00015df4   0x0000005c   Code   RO         2201    i.drv_i2c_s_clear_it_pending_bit  CVWL568.lib(drv_i2c_slave.o)
    0x00015e50   0x00015e50   0x00000034   Code   RO         2204    i.drv_i2c_s_enable_intr  CVWL568.lib(drv_i2c_slave.o)
    0x00015e84   0x00015e84   0x0000001c   Code   RO         2205    i.drv_i2c_s_get_fifo_status  CVWL568.lib(drv_i2c_slave.o)
    0x00015ea0   0x00015ea0   0x0000000c   Code   RO         2208    i.drv_i2c_s_set_callback  CVWL568.lib(drv_i2c_slave.o)
    0x00015eac   0x00015eac   0x00000020   Code   RO         2211    i.drv_i2c_s_write_data  CVWL568.lib(drv_i2c_slave.o)
    0x00015ecc   0x00015ecc   0x00000058   Code   RO         1622    i.drv_i2c_set_dma_irq_callback  CVWL568.lib(drv_i2c_dma.o)
    0x00015f24   0x00015f24   0x00000044   Code   RO         2212    i.drv_i2c_slave_init  CVWL568.lib(drv_i2c_slave.o)
    0x00015f68   0x00015f68   0x0000001c   Code   RO         1623    i.drv_i2c_slave_write_dma  CVWL568.lib(drv_i2c_dma.o)
    0x00015f84   0x00015f84   0x00000018   Code   RO         1639    i.drv_lcdc_config_bypass  CVWL568.lib(drv_lcdc.o)
    0x00015f9c   0x00015f9c   0x00000030   Code   RO         1640    i.drv_lcdc_config_ccm  CVWL568.lib(drv_lcdc.o)
    0x00015fcc   0x00015fcc   0x00000016   Code   RO         1641    i.drv_lcdc_config_disp_mode  CVWL568.lib(drv_lcdc.o)
    0x00015fe2   0x00015fe2   0x00000024   Code   RO         1642    i.drv_lcdc_config_dpi_polarity  CVWL568.lib(drv_lcdc.o)
    0x00016006   0x00016006   0x00000026   Code   RO         1643    i.drv_lcdc_config_dpi_timing  CVWL568.lib(drv_lcdc.o)
    0x0001602c   0x0001602c   0x00000016   Code   RO         1644    i.drv_lcdc_config_edpi_mode  CVWL568.lib(drv_lcdc.o)
    0x00016042   0x00016042   0x00000016   Code   RO         1645    i.drv_lcdc_config_endianness  CVWL568.lib(drv_lcdc.o)
    0x00016058   0x00016058   0x0000000c   Code   RO         1646    i.drv_lcdc_config_input_size  CVWL568.lib(drv_lcdc.o)
    0x00016064   0x00016064   0x0000001e   Code   RO         1647    i.drv_lcdc_config_int  CVWL568.lib(drv_lcdc.o)
    0x00016082   0x00016082   0x00000022   Code   RO         1648    i.drv_lcdc_config_int_single  CVWL568.lib(drv_lcdc.o)
    0x000160a4   0x000160a4   0x00000022   Code   RO         1649    i.drv_lcdc_config_overwrite  CVWL568.lib(drv_lcdc.o)
    0x000160c6   0x000160c6   0x0000000c   Code   RO         1650    i.drv_lcdc_config_overwrite_rgb  CVWL568.lib(drv_lcdc.o)
    0x000160d2   0x000160d2   0x0000001a   Code   RO         1651    i.drv_lcdc_config_partial_display_area  CVWL568.lib(drv_lcdc.o)
    0x000160ec   0x000160ec   0x00000022   Code   RO         1652    i.drv_lcdc_config_partial_display_enable  CVWL568.lib(drv_lcdc.o)
    0x0001610e   0x0001610e   0x00000028   Code   RO         1654    i.drv_lcdc_config_scale_up_coef  CVWL568.lib(drv_lcdc.o)
    0x00016136   0x00016136   0x0000000c   Code   RO         1655    i.drv_lcdc_config_scale_up_step  CVWL568.lib(drv_lcdc.o)
    0x00016142   0x00016142   0x0000004c   Code   RO         1656    i.drv_lcdc_config_src_parameter  CVWL568.lib(drv_lcdc.o)
    0x0001618e   0x0001618e   0x00000006   Code   RO         1657    i.drv_lcdc_config_thresh  CVWL568.lib(drv_lcdc.o)
    0x00016194   0x00016194   0x00000012   Code   RO         1658    i.drv_lcdc_ctrl_flow  CVWL568.lib(drv_lcdc.o)
    0x000161a6   0x000161a6   0x00000020   Code   RO         1660    i.drv_lcdc_enable_shadow_reg  CVWL568.lib(drv_lcdc.o)
    0x000161c6   0x000161c6   0x00000002   PAD
    0x000161c8   0x000161c8   0x00000034   Code   RO         1661    i.drv_lcdc_set_int  CVWL568.lib(drv_lcdc.o)
    0x000161fc   0x000161fc   0x00000014   Code   RO         1663    i.drv_lcdc_set_video_hw_mode  CVWL568.lib(drv_lcdc.o)
    0x00016210   0x00016210   0x00000020   Code   RO         1664    i.drv_lcdc_start    CVWL568.lib(drv_lcdc.o)
    0x00016230   0x00016230   0x0000000c   Code   RO         1698    i.drv_memc_clear_status  CVWL568.lib(drv_memc.o)
    0x0001623c   0x0001623c   0x00000040   Code   RO         1699    i.drv_memc_enable_irq  CVWL568.lib(drv_memc.o)
    0x0001627c   0x0001627c   0x0000000c   Code   RO         1700    i.drv_memc_gen_a_tear_signal  CVWL568.lib(drv_memc.o)
    0x00016288   0x00016288   0x00000012   Code   RO         1701    i.drv_memc_get_status  CVWL568.lib(drv_memc.o)
    0x0001629a   0x0001629a   0x00000010   Code   RO         1702    i.drv_memc_rate_transfer_sel  CVWL568.lib(drv_memc.o)
    0x000162aa   0x000162aa   0x0000000e   Code   RO         1703    i.drv_memc_sel_vsync  CVWL568.lib(drv_memc.o)
    0x000162b8   0x000162b8   0x00000014   Code   RO         1704    i.drv_memc_set_active_height  CVWL568.lib(drv_memc.o)
    0x000162cc   0x000162cc   0x0000000c   Code   RO         1705    i.drv_memc_set_data_mode  CVWL568.lib(drv_memc.o)
    0x000162d8   0x000162d8   0x00000010   Code   RO         1708    i.drv_memc_set_double_buffer  CVWL568.lib(drv_memc.o)
    0x000162e8   0x000162e8   0x00000012   Code   RO         1709    i.drv_memc_set_double_buffer_reverse  CVWL568.lib(drv_memc.o)
    0x000162fa   0x000162fa   0x00000010   Code   RO         1711    i.drv_memc_set_fs_en_conditions  CVWL568.lib(drv_memc.o)
    0x0001630a   0x0001630a   0x00000014   Code   RO         1712    i.drv_memc_set_inten  CVWL568.lib(drv_memc.o)
    0x0001631e   0x0001631e   0x00000002   PAD
    0x00016320   0x00016320   0x00000018   Code   RO         1713    i.drv_memc_set_lcdc_st_conditions  CVWL568.lib(drv_memc.o)
    0x00016338   0x00016338   0x0000001a   Code   RO         1714    i.drv_memc_set_ltpo_mode  CVWL568.lib(drv_memc.o)
    0x00016352   0x00016352   0x0000000e   Code   RO         1718    i.drv_memc_set_tear_mode  CVWL568.lib(drv_memc.o)
    0x00016360   0x00016360   0x00000028   Code   RO         1719    i.drv_memc_set_tear_waveform  CVWL568.lib(drv_memc.o)
    0x00016388   0x00016388   0x0000000e   Code   RO         1721    i.drv_memc_set_vidc_sync_cnt  CVWL568.lib(drv_memc.o)
    0x00016396   0x00016396   0x00000002   PAD
    0x00016398   0x00016398   0x00000008   Code   RO         1753    i.drv_param_init_get_ccm  CVWL568.lib(drv_param_init.o)
    0x000163a0   0x000163a0   0x00000014   Code   RO         1754    i.drv_param_init_get_scld_filter_h  CVWL568.lib(drv_param_init.o)
    0x000163b4   0x000163b4   0x00000014   Code   RO         1755    i.drv_param_init_get_scld_filter_v  CVWL568.lib(drv_param_init.o)
    0x000163c8   0x000163c8   0x00000008   Code   RO         1756    i.drv_param_init_get_sclu_filter  CVWL568.lib(drv_param_init.o)
    0x000163d0   0x000163d0   0x00000014   Code   RO         1757    i.drv_param_init_set_ccm  CVWL568.lib(drv_param_init.o)
    0x000163e4   0x000163e4   0x00000024   Code   RO         1759    i.drv_param_p2r_filter_init  CVWL568.lib(drv_param_init.o)
    0x00016408   0x00016408   0x00000054   Code   RO         2144    i.drv_phy_get_para  CVWL568.lib(drv_phy_common.o)
    0x0001645c   0x0001645c   0x00000020   Code   RO         1783    i.drv_pwm_out_enable  CVWL568.lib(drv_pwm.o)
    0x0001647c   0x0001647c   0x0000000c   Code   RO         1786    i.drv_pwm_out_set_control  CVWL568.lib(drv_pwm.o)
    0x00016488   0x00016488   0x0000000c   Code   RO         1787    i.drv_pwm_out_set_period  CVWL568.lib(drv_pwm.o)
    0x00016494   0x00016494   0x0000000c   Code   RO         1789    i.drv_pwm_out_set_threshold  CVWL568.lib(drv_pwm.o)
    0x000164a0   0x000164a0   0x00000020   Code   RO         2154    i.drv_pwr_set_cp_mode  CVWL568.lib(drv_pwr.o)
    0x000164c0   0x000164c0   0x00000018   Code   RO         2155    i.drv_pwr_set_pvd_mode  CVWL568.lib(drv_pwr.o)
    0x000164d8   0x000164d8   0x00000030   Code   RO         2156    i.drv_pwr_set_system_clk_src  CVWL568.lib(drv_pwr.o)
    0x00016508   0x00016508   0x0000001c   Code   RO         1324    i.drv_rx_phy_test_clear  CVWL568.lib(drv_dsi_rx.o)
    0x00016524   0x00016524   0x00000020   Code   RO         1325    i.drv_rx_phy_test_lock  CVWL568.lib(drv_dsi_rx.o)
    0x00016544   0x00016544   0x00000042   Code   RO         1327    i.drv_rx_phy_test_write  CVWL568.lib(drv_dsi_rx.o)
    0x00016586   0x00016586   0x0000000e   Code   RO         1328    i.drv_rx_phy_test_write_1_byte  CVWL568.lib(drv_dsi_rx.o)
    0x00016594   0x00016594   0x00000010   Code   RO         1329    i.drv_rx_phy_test_write_2_byte  CVWL568.lib(drv_dsi_rx.o)
    0x000165a4   0x000165a4   0x0000000a   Code   RO         1816    i.drv_rxbr_clear_pkt_buffer  CVWL568.lib(drv_rxbr.o)
    0x000165ae   0x000165ae   0x00000004   Code   RO         1817    i.drv_rxbr_clear_status0  CVWL568.lib(drv_rxbr.o)
    0x000165b2   0x000165b2   0x0000005a   Code   RO         1819    i.drv_rxbr_enable_irq  CVWL568.lib(drv_rxbr.o)
    0x0001660c   0x0001660c   0x00000014   Code   RO         1820    i.drv_rxbr_frame_drop_cfg  CVWL568.lib(drv_rxbr.o)
    0x00016620   0x00016620   0x0000003c   Code   RO         1821    i.drv_rxbr_get_clk  CVWL568.lib(drv_rxbr.o)
    0x0001665c   0x0001665c   0x00000004   Code   RO         1822    i.drv_rxbr_get_col_addr  CVWL568.lib(drv_rxbr.o)
    0x00016660   0x00016660   0x00000012   Code   RO          974    i.drv_rxbr_get_int_source  CVWL568.lib(hal_internal_vsync.o)
    0x00016672   0x00016672   0x00000004   Code   RO         1825    i.drv_rxbr_get_page_addr  CVWL568.lib(drv_rxbr.o)
    0x00016676   0x00016676   0x00000012   Code   RO          975    i.drv_rxbr_get_status0  CVWL568.lib(hal_internal_vsync.o)
    0x00016688   0x00016688   0x0000000c   Code   RO         1827    i.drv_rxbr_hline_rcv0_cfg  CVWL568.lib(drv_rxbr.o)
    0x00016694   0x00016694   0x00000008   Code   RO         1828    i.drv_rxbr_hline_rcv_cfg  CVWL568.lib(drv_rxbr.o)
    0x0001669c   0x0001669c   0x0000000c   Code   RO         1829    i.drv_rxbr_register_irq0_callback  CVWL568.lib(drv_rxbr.o)
    0x000166a8   0x000166a8   0x0000000c   Code   RO         1830    i.drv_rxbr_register_irq1_callback  CVWL568.lib(drv_rxbr.o)
    0x000166b4   0x000166b4   0x00000014   Code   RO         1831    i.drv_rxbr_set_ack_pkt_header  CVWL568.lib(drv_rxbr.o)
    0x000166c8   0x000166c8   0x000000cc   Code   RO         1832    i.drv_rxbr_set_cmd_filter  CVWL568.lib(drv_rxbr.o)
    0x00016794   0x00016794   0x00000014   Code   RO         1834    i.drv_rxbr_set_color_format  CVWL568.lib(drv_rxbr.o)
    0x000167a8   0x000167a8   0x00000014   Code   RO         1836    i.drv_rxbr_set_inten  CVWL568.lib(drv_rxbr.o)
    0x000167bc   0x000167bc   0x00000010   Code   RO         1837    i.drv_rxbr_set_ltpo_drop_th  CVWL568.lib(drv_rxbr.o)
    0x000167cc   0x000167cc   0x00000026   Code   RO         1839    i.drv_rxbr_set_usr_cfg  CVWL568.lib(drv_rxbr.o)
    0x000167f2   0x000167f2   0x00000008   Code   RO         1840    i.drv_rxbr_set_usr_col  CVWL568.lib(drv_rxbr.o)
    0x000167fa   0x000167fa   0x00000008   Code   RO         1841    i.drv_rxbr_set_usr_row  CVWL568.lib(drv_rxbr.o)
    0x00016802   0x00016802   0x00000002   PAD
    0x00016804   0x00016804   0x00000020   Code   RO         2242    i.drv_spi_m_read_data  CVWL568.lib(drv_spi_master.o)
    0x00016824   0x00016824   0x00000048   Code   RO         1909    i.drv_swire_set_int  CVWL568.lib(drv_swire.o)
    0x0001686c   0x0001686c   0x0000001c   Code   RO         1910    i.drv_swire_set_power_down  CVWL568.lib(drv_swire.o)
    0x00016888   0x00016888   0x0000000c   Code   RO         1925    i.drv_sys_cfg_clear_all_int  CVWL568.lib(drv_sys_cfg.o)
    0x00016894   0x00016894   0x00000028   Code   RO         1926    i.drv_sys_cfg_clear_pending  CVWL568.lib(drv_sys_cfg.o)
    0x000168bc   0x000168bc   0x00000018   Code   RO         1929    i.drv_sys_cfg_sel_ap_rst_lvl_trig  CVWL568.lib(drv_sys_cfg.o)
    0x000168d4   0x000168d4   0x0000001c   Code   RO         1930    i.drv_sys_cfg_sel_ap_rst_trig  CVWL568.lib(drv_sys_cfg.o)
    0x000168f0   0x000168f0   0x00000024   Code   RO         1931    i.drv_sys_cfg_sel_gpio_group  CVWL568.lib(drv_sys_cfg.o)
    0x00016914   0x00016914   0x00000024   Code   RO         1932    i.drv_sys_cfg_sel_int_trig  CVWL568.lib(drv_sys_cfg.o)
    0x00016938   0x00016938   0x00000010   Code   RO         1934    i.drv_sys_cfg_set_dma_rx_req  CVWL568.lib(drv_sys_cfg.o)
    0x00016948   0x00016948   0x00000010   Code   RO         1935    i.drv_sys_cfg_set_dma_tx_req  CVWL568.lib(drv_sys_cfg.o)
    0x00016958   0x00016958   0x00000024   Code   RO         1936    i.drv_sys_cfg_set_int  CVWL568.lib(drv_sys_cfg.o)
    0x0001697c   0x0001697c   0x0000001a   Code   RO         1960    i.drv_timer_clear_status_flags  CVWL568.lib(drv_timer.o)
    0x00016996   0x00016996   0x00000020   Code   RO         1961    i.drv_timer_enable  CVWL568.lib(drv_timer.o)
    0x000169b6   0x000169b6   0x00000002   PAD
    0x000169b8   0x000169b8   0x0000000c   Code   RO         1963    i.drv_timer_get_instance  CVWL568.lib(drv_timer.o)
    0x000169c4   0x000169c4   0x0000000e   Code   RO         1965    i.drv_timer_get_prescaler  CVWL568.lib(drv_timer.o)
    0x000169d2   0x000169d2   0x00000002   PAD
    0x000169d4   0x000169d4   0x00000010   Code   RO         1966    i.drv_timer_register_callback  CVWL568.lib(drv_timer.o)
    0x000169e4   0x000169e4   0x0000000c   Code   RO         1967    i.drv_timer_set_current_count  CVWL568.lib(drv_timer.o)
    0x000169f0   0x000169f0   0x00000048   Code   RO         1968    i.drv_timer_set_int  CVWL568.lib(drv_timer.o)
    0x00016a38   0x00016a38   0x0000000c   Code   RO         1969    i.drv_timer_set_match  CVWL568.lib(drv_timer.o)
    0x00016a44   0x00016a44   0x00000016   Code   RO         1970    i.drv_timer_set_prescaler  CVWL568.lib(drv_timer.o)
    0x00016a5a   0x00016a5a   0x0000000c   Code   RO         1407    i.drv_tx_phy_test_clear  CVWL568.lib(drv_dsi_tx.o)
    0x00016a66   0x00016a66   0x0000001c   Code   RO         1408    i.drv_tx_phy_test_enter  CVWL568.lib(drv_dsi_tx.o)
    0x00016a82   0x00016a82   0x0000001c   Code   RO         1409    i.drv_tx_phy_test_exit  CVWL568.lib(drv_dsi_tx.o)
    0x00016a9e   0x00016a9e   0x0000001a   Code   RO         1412    i.drv_tx_phy_test_write  CVWL568.lib(drv_dsi_tx.o)
    0x00016ab8   0x00016ab8   0x0000000e   Code   RO         1413    i.drv_tx_phy_test_write_1_byte  CVWL568.lib(drv_dsi_tx.o)
    0x00016ac6   0x00016ac6   0x00000012   Code   RO         1414    i.drv_tx_phy_test_write_2_byte  CVWL568.lib(drv_dsi_tx.o)
    0x00016ad8   0x00016ad8   0x00000022   Code   RO         1415    i.drv_tx_phy_test_write_code  CVWL568.lib(drv_dsi_tx.o)
    0x00016afa   0x00016afa   0x00000022   Code   RO         1416    i.drv_tx_phy_test_write_data  CVWL568.lib(drv_dsi_tx.o)
    0x00016b1c   0x00016b1c   0x00000008   Code   RO         1994    i.drv_vidc_clear_irq  CVWL568.lib(drv_vidc.o)
    0x00016b24   0x00016b24   0x00000018   Code   RO         1998    i.drv_vidc_enable   CVWL568.lib(drv_vidc.o)
    0x00016b3c   0x00016b3c   0x00000040   Code   RO         1999    i.drv_vidc_enable_irq  CVWL568.lib(drv_vidc.o)
    0x00016b7c   0x00016b7c   0x00000012   Code   RO         2001    i.drv_vidc_get_irq_status  CVWL568.lib(drv_vidc.o)
    0x00016b8e   0x00016b8e   0x00000002   PAD
    0x00016b90   0x00016b90   0x00000028   Code   RO         2005    i.drv_vidc_init_module_enable  CVWL568.lib(drv_vidc.o)
    0x00016bb8   0x00016bb8   0x0000000c   Code   RO         2006    i.drv_vidc_register_callback  CVWL568.lib(drv_vidc.o)
    0x00016bc4   0x00016bc4   0x00000006   Code   RO         2007    i.drv_vidc_reset    CVWL568.lib(drv_vidc.o)
    0x00016bca   0x00016bca   0x0000003c   Code   RO         2009    i.drv_vidc_set_dst_parameter  CVWL568.lib(drv_vidc.o)
    0x00016c06   0x00016c06   0x00000014   Code   RO         2013    i.drv_vidc_set_irqen  CVWL568.lib(drv_vidc.o)
    0x00016c1a   0x00016c1a   0x00000010   Code   RO         2014    i.drv_vidc_set_mirror  CVWL568.lib(drv_vidc.o)
    0x00016c2a   0x00016c2a   0x00000008   Code   RO         2017    i.drv_vidc_set_p2r_hcoef0  CVWL568.lib(drv_vidc.o)
    0x00016c32   0x00016c32   0x00000026   Code   RO         2018    i.drv_vidc_set_p2r_hinitb  CVWL568.lib(drv_vidc.o)
    0x00016c58   0x00016c58   0x00000026   Code   RO         2019    i.drv_vidc_set_p2r_hinitr  CVWL568.lib(drv_vidc.o)
    0x00016c7e   0x00016c7e   0x00000002   PAD
    0x00016c80   0x00016c80   0x00000018   Code   RO         2020    i.drv_vidc_set_pentile_swap  CVWL568.lib(drv_vidc.o)
    0x00016c98   0x00016c98   0x0000000a   Code   RO         2021    i.drv_vidc_set_pu_ctrl  CVWL568.lib(drv_vidc.o)
    0x00016ca2   0x00016ca2   0x00000010   Code   RO         2022    i.drv_vidc_set_rotation  CVWL568.lib(drv_vidc.o)
    0x00016cb2   0x00016cb2   0x0000000a   Code   RO         2023    i.drv_vidc_set_scld_hcoef0  CVWL568.lib(drv_vidc.o)
    0x00016cbc   0x00016cbc   0x0000000a   Code   RO         2024    i.drv_vidc_set_scld_hcoef1  CVWL568.lib(drv_vidc.o)
    0x00016cc6   0x00016cc6   0x00000012   Code   RO         2025    i.drv_vidc_set_scld_step  CVWL568.lib(drv_vidc.o)
    0x00016cd8   0x00016cd8   0x0000000a   Code   RO         2026    i.drv_vidc_set_scld_vcoef0  CVWL568.lib(drv_vidc.o)
    0x00016ce2   0x00016ce2   0x0000000a   Code   RO         2027    i.drv_vidc_set_scld_vcoef1  CVWL568.lib(drv_vidc.o)
    0x00016cec   0x00016cec   0x00000016   Code   RO         2028    i.drv_vidc_set_src_parameter  CVWL568.lib(drv_vidc.o)
    0x00016d02   0x00016d02   0x00000002   PAD
    0x00016d04   0x00016d04   0x00000010   Code   RO         2452    i.drv_wdg_clear_edge_flag  CVWL568.lib(drv_wdg.o)
    0x00016d14   0x00016d14   0x00000010   Code   RO         2455    i.drv_wdg_read_edge_flag  CVWL568.lib(drv_wdg.o)
    0x00016d24   0x00016d24   0x00000034   Code   RO         2458    i.drv_wdg_set_int   CVWL568.lib(drv_wdg.o)
    0x00016d58   0x00016d58   0x0000000a   Code   RO         1484    i.fls_clr_interrupt_flag  CVWL568.lib(drv_fls.o)
    0x00016d62   0x00016d62   0x00000014   Code   RO          941    i.fputc             CVWL568.lib(tau_log.o)
    0x00016d76   0x00016d76   0x00000002   PAD
    0x00016d78   0x00016d78   0x00000030   Code   RO          531    i.hal_dsi_rx_ctrl_create_handle  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016da8   0x00016da8   0x00000024   Code   RO          533    i.hal_dsi_rx_ctrl_deinit  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016dcc   0x00016dcc   0x00000084   Code   RO          535    i.hal_dsi_rx_ctrl_dsc_async_handler  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016e50   0x00016e50   0x00000028   Code   RO          537    i.hal_dsi_rx_ctrl_gen_a_tear_signal  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016e78   0x00016e78   0x00000028   Code   RO          539    i.hal_dsi_rx_ctrl_get_max_ret_size  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016ea0   0x00016ea0   0x00000098   Code   RO          541    i.hal_dsi_rx_ctrl_init  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016f38   0x00016f38   0x000002c8   Code   RO          542    i.hal_dsi_rx_ctrl_init_clk  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017200   0x00017200   0x000000c8   Code   RO          543    i.hal_dsi_rx_ctrl_init_dsi_rx  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000172c8   0x000172c8   0x0000013c   Code   RO          544    i.hal_dsi_rx_ctrl_init_memc  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017404   0x00017404   0x0000011c   Code   RO          545    i.hal_dsi_rx_ctrl_init_rxbr  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017520   0x00017520   0x0000022c   Code   RO          546    i.hal_dsi_rx_ctrl_init_vidc  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001774c   0x0001774c   0x0000003c   Code   RO          547    i.hal_dsi_rx_ctrl_pre_init_pps  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017788   0x00017788   0x000000f0   Code   RO          550    i.hal_dsi_rx_ctrl_send_ack_cmd  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017878   0x00017878   0x0000002c   Code   RO          552    i.hal_dsi_rx_ctrl_set_cus_esc_clk  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000178a4   0x000178a4   0x00000034   Code   RO          554    i.hal_dsi_rx_ctrl_set_cus_sync_line  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000178d8   0x000178d8   0x00000034   Code   RO          557    i.hal_dsi_rx_ctrl_set_hw_tear_mode  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001790c   0x0001790c   0x00000034   Code   RO          560    i.hal_dsi_rx_ctrl_set_sw_tear_mode  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017940   0x00017940   0x0000003c   Code   RO          563    i.hal_dsi_rx_ctrl_start  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001797c   0x0001797c   0x0000003c   Code   RO          564    i.hal_dsi_rx_ctrl_stop  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000179b8   0x000179b8   0x00000020   Code   RO          566    i.hal_dsi_rx_ctrl_toggle_resolution  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000179d8   0x000179d8   0x00000190   Code   RO          614    i.hal_dsi_tx_calc_video_chunks  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017b68   0x00017b68   0x0000050c   Code   RO          615    i.hal_dsi_tx_count_lane_rate  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018074   0x00018074   0x0000002c   Code   RO          616    i.hal_dsi_tx_ctrl_create_handle  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000180a0   0x000180a0   0x00000048   Code   RO          617    i.hal_dsi_tx_ctrl_deinit  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000180e8   0x000180e8   0x0000004c   Code   RO          618    i.hal_dsi_tx_ctrl_enter_init_panel_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018134   0x00018134   0x00000028   Code   RO          620    i.hal_dsi_tx_ctrl_exit_init_panel_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001815c   0x0001815c   0x000000a4   Code   RO          622    i.hal_dsi_tx_ctrl_init  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018200   0x00018200   0x00000024   Code   RO          623    i.hal_dsi_tx_ctrl_init_clk  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018224   0x00018224   0x0000000c   Code   RO          624    i.hal_dsi_tx_ctrl_panel_reset_pin  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018230   0x00018230   0x00000020   Code   RO          627    i.hal_dsi_tx_ctrl_set_ccm  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018250   0x00018250   0x00000014   Code   RO          632    i.hal_dsi_tx_ctrl_set_overwrite_rgb  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018264   0x00018264   0x00000010   Code   RO          633    i.hal_dsi_tx_ctrl_set_partial_disp  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018274   0x00018274   0x00000024   Code   RO          634    i.hal_dsi_tx_ctrl_set_partial_disp_area  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018298   0x00018298   0x0000006c   Code   RO          636    i.hal_dsi_tx_ctrl_start  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018304   0x00018304   0x00000044   Code   RO          637    i.hal_dsi_tx_ctrl_stop  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018348   0x00018348   0x000000d8   Code   RO          638    i.hal_dsi_tx_ctrl_write_array_cmd  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018420   0x00018420   0x000000b0   Code   RO          639    i.hal_dsi_tx_ctrl_write_cmd  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000184d0   0x000184d0   0x00000044   Code   RO          640    i.hal_dsi_tx_init_data_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018514   0x00018514   0x00000030   Code   RO          641    i.hal_dsi_tx_init_dpi_cfg  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018544   0x00018544   0x00000020   Code   RO          642    i.hal_dsi_tx_init_interrupt  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018564   0x00018564   0x00000020   Code   RO          643    i.hal_dsi_tx_init_phy_cfg  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018584   0x00018584   0x00000094   Code   RO          644    i.hal_dsi_tx_init_remains  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018618   0x00018618   0x00000058   Code   RO          645    i.hal_dsi_tx_init_video_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018670   0x00018670   0x00000070   Code   RO          646    i.hal_dsi_tx_phy_test_get_data  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000186e0   0x000186e0   0x000000f4   Code   RO          647    i.hal_dsi_tx_phy_test_setup  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000187d4   0x000187d4   0x00000044   Code   RO          648    i.hal_dsi_tx_send_cmd  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018818   0x00018818   0x00000018   Code   RO          706    i.hal_gpio_ctrl_eint  CVWL568.lib(hal_gpio.o)
    0x00018830   0x00018830   0x00000012   Code   RO          707    i.hal_gpio_get_input_data  CVWL568.lib(hal_gpio.o)
    0x00018842   0x00018842   0x00000002   PAD
    0x00018844   0x00018844   0x00000040   Code   RO          710    i.hal_gpio_init_eint  CVWL568.lib(hal_gpio.o)
    0x00018884   0x00018884   0x00000028   Code   RO          712    i.hal_gpio_init_output  CVWL568.lib(hal_gpio.o)
    0x000188ac   0x000188ac   0x00000018   Code   RO          713    i.hal_gpio_reg_eint_cb  CVWL568.lib(hal_gpio.o)
    0x000188c4   0x000188c4   0x00000050   Code   RO          714    i.hal_gpio_set_ap_reset_int  CVWL568.lib(hal_gpio.o)
    0x00018914   0x00018914   0x00000060   Code   RO          716    i.hal_gpio_set_mode  CVWL568.lib(hal_gpio.o)
    0x00018974   0x00018974   0x00000008   Code   RO          717    i.hal_gpio_set_output_data  CVWL568.lib(hal_gpio.o)
    0x0001897c   0x0001897c   0x00000020   Code   RO          719    i.hal_gpio_set_pull_state  CVWL568.lib(hal_gpio.o)
    0x0001899c   0x0001899c   0x0000006c   Code   RO          856    i.hal_i2c_m_dma_init  CVWL568.lib(hal_i2c_master.o)
    0x00018a08   0x00018a08   0x00000020   Code   RO          857    i.hal_i2c_m_dma_read  CVWL568.lib(hal_i2c_master.o)
    0x00018a28   0x00018a28   0x0000001c   Code   RO          858    i.hal_i2c_m_dma_write  CVWL568.lib(hal_i2c_master.o)
    0x00018a44   0x00018a44   0x0000000c   Code   RO          860    i.hal_i2c_m_transfer_complate  CVWL568.lib(hal_i2c_master.o)
    0x00018a50   0x00018a50   0x00000020   Code   RO          861    i.hal_i2c_master_irq_callback  CVWL568.lib(hal_i2c_master.o)
    0x00018a70   0x00018a70   0x00000010   Code   RO          873    i.hal_i2c_s_dma_user_callback  CVWL568.lib(hal_i2c_slave.o)
    0x00018a80   0x00018a80   0x00000038   Code   RO          874    i.hal_i2c_s_dma_write  CVWL568.lib(hal_i2c_slave.o)
    0x00018ab8   0x00018ab8   0x0000006c   Code   RO          876    i.hal_i2c_s_init    CVWL568.lib(hal_i2c_slave.o)
    0x00018b24   0x00018b24   0x00000014   Code   RO          877    i.hal_i2c_s_nonblocking_read  CVWL568.lib(hal_i2c_slave.o)
    0x00018b38   0x00018b38   0x0000000c   Code   RO          884    i.hal_i2c_s_set_transfer  CVWL568.lib(hal_i2c_slave.o)
    0x00018b44   0x00018b44   0x00000118   Code   RO          887    i.hal_i2c_slave_irq_callback  CVWL568.lib(hal_i2c_slave.o)
    0x00018c5c   0x00018c5c   0x000000e4   Code   RO          977    i.hal_internal_init_memc  CVWL568.lib(hal_internal_vsync.o)
    0x00018d40   0x00018d40   0x00000010   Code   RO          978    i.hal_internal_sync_get_fb_setting  CVWL568.lib(hal_internal_vsync.o)
    0x00018d50   0x00018d50   0x00000214   Code   RO          979    i.hal_internal_sync_input_resolution_change  CVWL568.lib(hal_internal_vsync.o)
    0x00018f64   0x00018f64   0x0000001c   Code   RO          981    i.hal_internal_vsync_deinit  CVWL568.lib(hal_internal_vsync.o)
    0x00018f80   0x00018f80   0x00000018   Code   RO          983    i.hal_internal_vsync_get_sync_line  CVWL568.lib(hal_internal_vsync.o)
    0x00018f98   0x00018f98   0x000000fc   Code   RO          985    i.hal_internal_vsync_init_rx  CVWL568.lib(hal_internal_vsync.o)
    0x00019094   0x00019094   0x000000b0   Code   RO          986    i.hal_internal_vsync_init_tx  CVWL568.lib(hal_internal_vsync.o)
    0x00019144   0x00019144   0x0000011c   Code   RO          987    i.hal_internal_vsync_set_auto_hw_filter  CVWL568.lib(hal_internal_vsync.o)
    0x00019260   0x00019260   0x00000014   Code   RO          989    i.hal_internal_vsync_set_rx_state  CVWL568.lib(hal_internal_vsync.o)
    0x00019274   0x00019274   0x0000001c   Code   RO          990    i.hal_internal_vsync_set_sync_line  CVWL568.lib(hal_internal_vsync.o)
    0x00019290   0x00019290   0x00000044   Code   RO          991    i.hal_internal_vsync_set_tear_mode  CVWL568.lib(hal_internal_vsync.o)
    0x000192d4   0x000192d4   0x00000040   Code   RO          992    i.hal_internal_vsync_set_tx_state  CVWL568.lib(hal_internal_vsync.o)
    0x00019314   0x00019314   0x00000024   Code   RO          649    i.hal_lcdc_config_ccm  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00019338   0x00019338   0x00000048   Code   RO          650    i.hal_lcdc_config_remains  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00019380   0x00019380   0x00000014   Code   RO          651    i.hal_lcdc_config_rgb_to_pentile  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00019394   0x00019394   0x00000164   Code   RO          652    i.hal_lcdc_config_upscaler  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000194f8   0x000194f8   0x00000040   Code   RO          653    i.hal_lcdc_init_cfg  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00019538   0x00019538   0x00000134   Code   RO          654    i.hal_lcdc_init_clk  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001966c   0x0001966c   0x00000040   Code   RO          655    i.hal_lcdc_init_interrupt  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000196ac   0x000196ac   0x00000068   Code   RO          755    i.hal_pwm_out_config_all  CVWL568.lib(hal_pwm.o)
    0x00019714   0x00019714   0x0000000c   Code   RO          757    i.hal_pwm_out_init  CVWL568.lib(hal_pwm.o)
    0x00019720   0x00019720   0x0000000e   Code   RO          909    i.hal_spi_m_clear_rxfifo  CVWL568.lib(hal_spi_master.o)
    0x0001972e   0x0001972e   0x00000016   Code   RO          792    i.hal_swire_open    CVWL568.lib(hal_swire.o)
    0x00019744   0x00019744   0x00000008   Code   RO          808    i.hal_system_enable_systick  CVWL568.lib(hal_system.o)
    0x0001974c   0x0001974c   0x0000007c   Code   RO          813    i.hal_system_init   CVWL568.lib(hal_system.o)
    0x000197c8   0x000197c8   0x0000001c   Code   RO          814    i.hal_system_init_console  CVWL568.lib(hal_system.o)
    0x000197e4   0x000197e4   0x00000008   Code   RO          817    i.hal_system_set_pvd  CVWL568.lib(hal_system.o)
    0x000197ec   0x000197ec   0x00000008   Code   RO          818    i.hal_system_set_vcc  CVWL568.lib(hal_system.o)
    0x000197f4   0x000197f4   0x00000022   Code   RO          844    i.hal_timer_init    CVWL568.lib(hal_timer.o)
    0x00019816   0x00019816   0x00000002   PAD
    0x00019818   0x00019818   0x00000054   Code   RO          845    i.hal_timer_start   CVWL568.lib(hal_timer.o)
    0x0001986c   0x0001986c   0x00000028   Code   RO          846    i.hal_timer_stop    CVWL568.lib(hal_timer.o)
    0x00019894   0x00019894   0x0000008c   Code   RO          952    i.hal_uart_init     CVWL568.lib(hal_uart.o)
    0x00019920   0x00019920   0x00000010   Code   RO          955    i.hal_uart_transmit_blocking  CVWL568.lib(hal_uart.o)
    0x00019930   0x00019930   0x00000110   Code   RO         2104    i.handle_init       CVWL568.lib(irq_redirect .o)
    0x00019a40   0x00019a40   0x00000070   Code   RO          114    i.init_mipi_tx      ap_demo.o
    0x00019ab0   0x00019ab0   0x000000fc   Code   RO          115    i.init_panel        ap_demo.o
    0x00019bac   0x00019bac   0x0000000a   Code   RO            3    i.main              main.o
    0x00019bb6   0x00019bb6   0x00000002   PAD
    0x00019bb8   0x00019bb8   0x000000b0   Code   RO          116    i.open_mipi_rx      ap_demo.o
    0x00019c68   0x00019c68   0x0000006c   Code   RO          117    i.pps_update_handle  ap_demo.o
    0x00019cd4   0x00019cd4   0x000003f4   Code   RO          993    i.rx_get_dcs_packet_data  CVWL568.lib(hal_internal_vsync.o)
    0x0001a0c8   0x0001a0c8   0x00000140   Code   RO          994    i.rx_partial_update  CVWL568.lib(hal_internal_vsync.o)
    0x0001a208   0x0001a208   0x0000008c   Code   RO          995    i.rx_receive_packet  CVWL568.lib(hal_internal_vsync.o)
    0x0001a294   0x0001a294   0x00000180   Code   RO          996    i.rx_receive_pps    CVWL568.lib(hal_internal_vsync.o)
    0x0001a414   0x0001a414   0x000000a4   Code   RO          997    i.rxbr_irq0_callback  CVWL568.lib(hal_internal_vsync.o)
    0x0001a4b8   0x0001a4b8   0x00000170   Code   RO          998    i.rxbr_irq1_callback  CVWL568.lib(hal_internal_vsync.o)
    0x0001a628   0x0001a628   0x0000008c   Code   RO          999    i.soft_gen_te       CVWL568.lib(hal_internal_vsync.o)
    0x0001a6b4   0x0001a6b4   0x00000030   Code   RO          118    i.soft_timer3_cb    ap_demo.o
    0x0001a6e4   0x0001a6e4   0x000000b4   Code   RO         1000    i.vidc_callback     CVWL568.lib(hal_internal_vsync.o)
    0x0001a798   0x0001a798   0x000000d0   Code   RO         1001    i.vpre_err_reset    CVWL568.lib(hal_internal_vsync.o)
    0x0001a868   0x0001a868   0x0000019c   Code   RO         1002    i.vsync_set_te_mode  CVWL568.lib(hal_internal_vsync.o)
    0x0001aa04   0x0001aa04   0x0000339c   Data   RO          120    .constdata          ap_demo.o
    0x0001dda0   0x0001dda0   0x00000932   Data   RO          271    .constdata          app_tp_for_custom_s8.o
    0x0001e6d2   0x0001e6d2   0x00000001   Data   RO          284    .constdata          app_tp_for_custom_s8.o
    0x0001e6d3   0x0001e6d3   0x00000001   PAD
    0x0001e6d4   0x0001e6d4   0x00000104   Data   RO          657    .constdata          CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001e7d8   0x0001e7d8   0x000000d2   Data   RO          722    .constdata          CVWL568.lib(hal_gpio.o)
    0x0001e8aa   0x0001e8aa   0x00000002   PAD
    0x0001e8ac   0x0001e8ac   0x00000008   Data   RO         1760    .constdata          CVWL568.lib(drv_param_init.o)
    0x0001e8b4   0x0001e8b4   0x00000020   Data   RO         1972    .constdata          CVWL568.lib(drv_timer.o)
    0x0001e8d4   0x0001e8d4   0x00000138   Data   RO         2145    .constdata          CVWL568.lib(drv_phy_common.o)
    0x0001ea0c   0x0001ea0c   0x00000048   Data   RO          568    .conststring        CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001ea54   0x0001ea54   0x00000134   Data   RO         1004    .conststring        CVWL568.lib(hal_internal_vsync.o)
    0x0001eb88   0x0001eb88   0x00000030   Data   RO         2867    Region$$Table       anon$$obj.o


    Execution Region RW_RAM1 (Exec base: 0x00070000, Load base: 0x0001ebb8, Size: 0x00000000, Max: 0x000000f0, ABSOLUTE)

    **** No section assigned to this execution region ****


    Execution Region RW_RAM2 (Exec base: 0x00070100, Load base: 0x0001ebb8, Size: 0x000000c0, Max: 0x000000d0, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00070100        -       0x000000c0   Zero   RW         2105    .ARM.__AT_0x00070100  CVWL568.lib(irq_redirect .o)


    Execution Region RW_RAM3 (Exec base: 0x000701d0, Load base: 0x0001ebb8, Size: 0x000036a0, Max: 0x00007e30, ABSOLUTE, COMPRESSED[0x000003c8])

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x000701d0   COMPRESSED   0x00000030   Data   RW          121    .data               ap_demo.o
    0x00070200   COMPRESSED   0x000000e4   Data   RW          285    .data               app_tp_for_custom_s8.o
    0x000702e4   COMPRESSED   0x00000001   Data   RW          288    .data               app_tp_for_custom_s8.o
    0x000702e5   COMPRESSED   0x00000001   Data   RW          289    .data               app_tp_for_custom_s8.o
    0x000702e6   COMPRESSED   0x00000001   Data   RW          294    .data               app_tp_for_custom_s8.o
    0x000702e7   COMPRESSED   0x00000003   Data   RW          295    .data               app_tp_for_custom_s8.o
    0x000702ea   COMPRESSED   0x00000005   Data   RW          296    .data               app_tp_for_custom_s8.o
    0x000702ef   COMPRESSED   0x00000001   PAD
    0x000702f0   COMPRESSED   0x00000030   Data   RW          306    .data               app_tp_for_custom_s8.o
    0x00070320   COMPRESSED   0x00000030   Data   RW          377    .data               app_tp_transfer.o
    0x00070350   COMPRESSED   0x00000008   Data   RW          569    .data               CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00070358   COMPRESSED   0x00000001   Data   RW          658    .data               CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00070359   COMPRESSED   0x00000001   Data   RW          862    .data               CVWL568.lib(hal_i2c_master.o)
    0x0007035a   COMPRESSED   0x00000002   PAD
    0x0007035c   COMPRESSED   0x0000001c   Data   RW          888    .data               CVWL568.lib(hal_i2c_slave.o)
    0x00070378   COMPRESSED   0x00000004   Data   RW         1005    .data               CVWL568.lib(hal_internal_vsync.o)
    0x0007037c   COMPRESSED   0x00000012   Data   RW         1084    .data               CVWL568.lib(norflash.o)
    0x0007038e   COMPRESSED   0x00000002   PAD
    0x00070390   COMPRESSED   0x0000000c   Data   RW         1148    .data               CVWL568.lib(drv_common.o)
    0x0007039c   COMPRESSED   0x00000004   Data   RW         1587    .data               CVWL568.lib(drv_gpio.o)
    0x000703a0   COMPRESSED   0x00000008   Data   RW         1625    .data               CVWL568.lib(drv_i2c_dma.o)
    0x000703a8   COMPRESSED   0x000004a4   Data   RW         1761    .data               CVWL568.lib(drv_param_init.o)
    0x0007084c   COMPRESSED   0x0000000c   Data   RW         1790    .data               CVWL568.lib(drv_pwm.o)
    0x00070858   COMPRESSED   0x00000008   Data   RW         1843    .data               CVWL568.lib(drv_rxbr.o)
    0x00070860   COMPRESSED   0x00000008   Data   RW         1912    .data               CVWL568.lib(drv_swire.o)
    0x00070868   COMPRESSED   0x00000001   Data   RW         1937    .data               CVWL568.lib(drv_sys_cfg.o)
    0x00070869   COMPRESSED   0x00000003   PAD
    0x0007086c   COMPRESSED   0x00000004   Data   RW         2030    .data               CVWL568.lib(drv_vidc.o)
    0x00070870   COMPRESSED   0x00000004   Data   RW         2179    .data               CVWL568.lib(drv_i2c_master.o)
    0x00070874   COMPRESSED   0x00000008   Data   RW         2213    .data               CVWL568.lib(drv_i2c_slave.o)
    0x0007087c   COMPRESSED   0x00000004   Data   RW         2247    .data               CVWL568.lib(drv_spi_master.o)
    0x00070880   COMPRESSED   0x0000000c   Data   RW         2270    .data               CVWL568.lib(drv_chip_info.o)
    0x0007088c   COMPRESSED   0x00000008   Data   RW         2393    .data               CVWL568.lib(drv_uart.o)
    0x00070894   COMPRESSED   0x00000008   Data   RW         2459    .data               CVWL568.lib(drv_wdg.o)
    0x0007089c   COMPRESSED   0x00000004   Data   RW         2845    .data               mc_p.l(stdout.o)
    0x000708a0        -       0x00000190   Zero   RW          376    .bss                app_tp_transfer.o
    0x00070a30        -       0x000000c0   Zero   RW          567    .bss                CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00070af0        -       0x00000048   Zero   RW          656    .bss                CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00070b38        -       0x00000100   Zero   RW          942    .bss                CVWL568.lib(tau_log.o)
    0x00070c38        -       0x000000d0   Zero   RW          957    .bss                CVWL568.lib(hal_uart.o)
    0x00070d08        -       0x00000958   Zero   RW         1003    .bss                CVWL568.lib(hal_internal_vsync.o)
    0x00071660        -       0x00001030   Zero   RW         1131    .bss                CVWL568.lib(dcs_packet_fifo.o)
    0x00072690        -       0x0000001c   Zero   RW         1275    .bss                CVWL568.lib(drv_dma.o)
    0x000726ac        -       0x00000040   Zero   RW         1586    .bss                CVWL568.lib(drv_gpio.o)
    0x000726ec        -       0x00000140   Zero   RW         1624    .bss                CVWL568.lib(drv_i2c_dma.o)
    0x0007282c        -       0x00000020   Zero   RW         1971    .bss                CVWL568.lib(drv_timer.o)
    0x0007284c        -       0x00000020   Zero   RW         2314    .bss                CVWL568.lib(hal_spi_slave.o)
    0x0007286c   COMPRESSED   0x00000004   PAD
    0x00072870        -       0x00001000   Zero   RW          520    STACK               startup_armcm0.o


==============================================================================

Image component sizes


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Object Name

      6822        786      13212         48          0      33666   ap_demo.o
      1460         32       2355        287          0      13476   app_tp_for_custom_s8.o
      1092        114          0         48        400      11951   app_tp_transfer.o
        28          4          0          0          0        429   board.o
        10          0          0          0          0       9483   main.o
       120         18        192          0       4096       2012   startup_armcm0.o

    ----------------------------------------------------------------------
      9536        954      15808        384       4496      71017   Object Totals
         0          0         48          0          0          0   (incl. Generated)
         4          0          1          1          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Member Name

       216         32          0          0       4144        252   dcs_packet_fifo.o
       296         96          0         12          0        256   drv_chip_info.o
       192         82         20         12          0        264   drv_common.o
       432         94          0          0          0       1260   drv_crgu.o
       410         28          0          0         28        796   drv_dma.o
       232         28          0          0          0        340   drv_dsc_dec.o
      1628        488          0          0          0       1328   drv_dsi_rx.o
      1282        118          0          0          0       2480   drv_dsi_tx.o
       118          0          0          0          0        256   drv_efuse.o
        10          0          0          0          0         60   drv_fls.o
       784        112          0          4         64       1236   drv_gpio.o
       588         88          0          8        320        624   drv_i2c_dma.o
       360         86          0          4          0        456   drv_i2c_master.o
       324         74          0          8          0        516   drv_i2c_slave.o
       682          6          0          0          0       1444   drv_lcdc.o
       492         28          0          0          0       1112   drv_memc.o
       112         36          8       1188          0        376   drv_param_init.o
        84          8        312          0          0         68   drv_phy_common.o
       140         32          0         12          0        316   drv_pwm.o
       104         24          0          0          0        180   drv_pwr.o
       682         66          0          8          0       1448   drv_rxbr.o
       104         24          0          4          0        188   drv_spi_master.o
       132         16          0          8          0        200   drv_swire.o
       300         64          0          1          0        628   drv_sys_cfg.o
       378         28         32          0         32        872   drv_timer.o
       698         18          0          8          0        680   drv_uart.o
       510         28          0          4          0       1452   drv_vidc.o
       128         18          0          8          0        256   drv_wdg.o
      3194        372         72          8        192       1536   hal_dsi_rx_ctrl.o
      4568        306        260          1         72       2472   hal_dsi_tx_ctrl.o
       418         44        210          0          0        684   hal_gpio.o
       212         40          0          1          0        340   hal_i2c_master.o
       492         70          0         28          0        400   hal_i2c_slave.o
      6216       1478        308          4       2392       2132   hal_internal_vsync.o
       116          4          0          0          0        148   hal_pwm.o
        14          0          0          0          0         68   hal_spi_master.o
       232         20          0          0         32        136   hal_spi_slave.o
        22          0          0          0          0         68   hal_swire.o
       176         28          0          0          0        340   hal_system.o
       158          6          0          0          0        212   hal_timer.o
       156         18          0          0        208        144   hal_uart.o
      1076        324          0          0        192       1980   irq_redirect .o
        48         10          0         18          0         68   norflash.o
        58          0          0          0          0        128   tau_delay.o
        60         10          0          0        256        156   tau_log.o
       200         20          0          0          0         76   ceil.o
        86          0          0          0          0          0   __dczerorl2.o
         0          0          0          0          0          0   entry.o
         0          0          0          0          0          0   entry10a.o
         0          0          0          0          0          0   entry11a.o
         8          4          0          0          0          0   entry2.o
         4          0          0          0          0          0   entry5.o
         0          0          0          0          0          0   entry7b.o
         0          0          0          0          0          0   entry8b.o
         8          4          0          0          0          0   entry9a.o
        30          0          0          0          0          0   handlers.o
        40          0          0          0          0         72   idiv.o
        36          8          0          0          0         68   init.o
         0          0          0          0          0          0   iusefp.o
        32          0          0          0          0         68   llshl.o
        38          0          0          0          0         68   llsshr.o
        34          0          0          0          0         68   llushr.o
        36          0          0          0          0         60   memcpya.o
        36          0          0          0          0        100   memseta.o
      2298        104          0          0          0        544   printfa.o
         0          0          0          4          0          0   stdout.o
        44          0          0          0          0         72   uidiv.o
        96          0          0          0          0         84   uldiv.o
        40          2          0          0          0         68   cdrcmple.o
        20          0          0          0          0         68   cfrcmple.o
       356          4          0          0          0        140   dadd.o
       240          6          0          0          0         84   ddiv.o
       236          0          0          0          0        216   depilogue.o
        72         10          0          0          0         72   dfixi.o
        60         10          0          0          0         68   dfixui.o
        64         10          0          0          0         68   dfixul.o
        28          4          0          0          0         68   dfltui.o
       208          6          0          0          0         88   dmul.o
        40          0          0          0          0         60   f2d.o
       178          0          0          0          0        108   fadd.o
       124          0          0          0          0         72   fdiv.o
       130          0          0          0          0        144   fepilogue.o
        50          0          0          0          0         60   ffixi.o
        40          0          0          0          0         60   ffixui.o
        22          0          0          0          0         68   fflti.o
        14          0          0          0          0         68   ffltui.o
       122          0          0          0          0         72   fmul.o
        24          0          0          0          0         60   fscalb.o

    ----------------------------------------------------------------------
     33776       4644       1224       1360       7936      33348   Library Totals
        48          0          2          7          4          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Name

     28634       4452       1222       1349       7932      30356   CVWL568.lib
       200         20          0          0          0         76   m_ps.l
      2826        120          0          4          0       1204   mc_p.l
      2068         52          0          0          0       1712   mf_p.l

    ----------------------------------------------------------------------
     33776       4644       1224       1360       7936      33348   Library Totals

    ----------------------------------------------------------------------

==============================================================================


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   

     43312       5598      17032       1744      12432      81297   Grand Totals
     43312       5598      17032        968      12432      81297   ELF Image Totals (compressed)
     43312       5598      17032        968          0          0   ROM Totals

==============================================================================

    Total RO  Size (Code + RO Data)                60344 (  58.93kB)
    Total RW  Size (RW Data + ZI Data)             14176 (  13.84kB)
    Total ROM Size (Code + RO Data + RW Data)      61312 (  59.88kB)

==============================================================================

