#

##

##

##

##

##

##

    礦ision Build Log
    Tool Versions:
    IDE-Version: μVision V5.28.0.0
    Copyright (C) 2019 ARM Ltd and ARM Germany GmbH. All rights reserved.
    License Information: HAHA Markin, HAHA, LIC=VGXG8-3CKFQ-63XMB-246PQ-J4CUG-RTS7K

    Tool Versions:
    Toolchain:       MDK-ARM Plus  Version: 5.28.0.0
    Toolchain Path:  C:\Keil_v5\ARM\ARMCC\Bin
    C Compiler:      Armcc.exe V5.06 update 6 (build 750)
    Assembler:       Armasm.exe V5.06 update 6 (build 750)
    Linker/Locator:  ArmLink.exe V5.06 update 6 (build 750)
    Library Manager: ArmAr.exe V5.06 update 6 (build 750)
    Hex Converter:   FromElf.exe V5.06 update 6 (build 750)
    CPU DLL:         SARMCM3.DLL V5.28.0.0
    Dialog DLL:      DARMCM1.DLL V1.19.2.0
    Target DLL:      UL2CM3.DLL V1.162.16.0
    Dialog DLL:      TARMCM1.DLL V1.14.1.0

    Project:
    D:\Custom\博创晶彩\WL568_S21_NT37701AH_HX628\调试代码\WL568_S21_NT37701AH_HX628_20230306(开机屏幕底部偶发花屏)\WL568_S21_NT37701AH_HX628_20230301(TouchDelay)(DING)(1)\WL568_S21_NT37701AH_HX628_20230301(TouchDelay)\project\ISP568.uvprojx
    Project File Date:  03/01/2023

    Output:
    *** Using Compiler 'V5.06 update 6 (build 750)', folder: 'C:\Keil_v5\ARM\ARMCC\Bin'
    Rebuild target 'ISP568'
    creating preprocessor file for main.c...
    compiling main.c...
    creating preprocessor file for ap_demo.c...
    compiling ap_demo.c...
    ..\src\app\demo\ap_demo.c(4726): warning:  #167-D: argument of type "const uint8_t *" is incompatible with parameter of type "uint8_t *"
            send_panel_init_code(sizeof(panel_init_code), panel_init_code);
    ..\src\app\demo\ap_demo.c(128): warning:  #177-D: variable "swire_num_bak"  was declared but never referenced
      static uint8_t swire_num_bak=SWIRE_DEFAULT_NUM;
    ..\src\app\demo\ap_demo.c(133): warning:  #550-D: variable "g_exit_sleep_mode"  was set but never used
      static bool g_exit_sleep_mode = false;
    ..\src\app\demo\ap_demo.c(139): warning:  #550-D: variable "panel_display_done"  was set but never used
      static bool panel_display_done = false;
    ..\src\app\demo\ap_demo.c(4893): warning:  #177-D: function "swire_init"  was declared but never referenced
      static void swire_init()
    ..\src\app\demo\ap_demo.c(1513): warning:  #550-D: variable "value_reg_df"  was set but never used
      static uint32_t value_reg_df =0;
    ..\src\app\demo\ap_demo.c(1514): warning:  #177-D: variable "value_blue"  was declared but never referenced
      static uint8_t value_blue =0;
    ..\src\app\demo\ap_demo.c(1515): warning:  #177-D: variable "blue_flag"  was declared but never referenced
      static uint8_t blue_flag =0;
    ..\src\app\demo\ap_demo.c(1836): warning:  #177-D: function "ap_get_reg_ca"  was declared but never referenced
      static bool ap_get_reg_ca(hal_dsi_rx_ctrl_handle_t *handler, hal_dcs_packet_t *dcs_packet)
    ..\src\app\demo\ap_demo.c: 9 warnings, 0 errors
    creating preprocessor file for app_tp_transfer.c...
    compiling app_tp_transfer.c...
    ..\src\app\demo\app_tp_transfer.c(97): warning:  #177-D: variable "i"  was declared but never referenced
            uint8_t i = 1;
    ..\src\app\demo\app_tp_transfer.c(98): warning:  #177-D: variable "j"  was declared but never referenced
            uint8_t j = 1;
    ..\src\app\demo\app_tp_transfer.c(484): warning:  #177-D: variable "ii"  was declared but never referenced
            uint8_t ii;
    ..\src\app\demo\app_tp_transfer.c(735): warning:  #177-D: variable "temp_len"  was declared but never referenced
            uint8_t temp_len=0;
    ..\src\app\demo\app_tp_transfer.c(738): warning:  #550-D: variable "screen_int_transfer_buffer_ready"  was set but never used
            static bool    screen_int_transfer_buffer_ready = true;  //发送 buffer 是否已准备好
    ..\src\app\demo\app_tp_transfer.c(30): warning:  #550-D: variable "s_screen_int_transfer_status"  was set but never used
      static bool    s_screen_int_transfer_status = false;   //记录是否已经开始通信
    ..\src\app\demo\app_tp_transfer.c: 6 warnings, 0 errors
    creating preprocessor file for board.c...
    compiling board.c...
    assembling startup_ARMCM0.s...
    linking...
    Program Size: Code=44456 RO-data=15940 RW-data=2344 ZI-data=12408
    FromELF: creating hex file...
    After Build - User command #1: fromelf  --bin  -o  .\Objects\WL568_S21_NT37701.bin  .\Objects\WL568_S21_NT37701.axf
    ".\Objects\WL568_S21_NT37701.axf" - 0 Error(s), 15 Warning(s).

    Software Packages used:

    Package Vendor: ARM
                    http://www.keil.com/pack/ARM.CMSIS.5.5.1.pack
                    ARM.CMSIS.5.5.1
                    CMSIS (Cortex Microcontroller Software Interface Standard)
       * Component: CORE Version: 5.2.0

    Collection of Component include folders:
      .\RTE\_ISP568
      C:\Users\Markin\AppData\Local\Arm\Packs\ARM\CMSIS\5.5.1\CMSIS\Core\Include
      C:\Users\Markin\AppData\Local\Arm\Packs\ARM\CMSIS\5.5.1\Device\ARM\ARMCM0\Include

    Collection of Component Files used:

       * Component: ARM::CMSIS:CORE:5.2.0
    Build Time Elapsed:  00:00:02