Component: ARM Compiler 5.06 update 6 (build 750) Tool: armlink [4d35ed]

==============================================================================

Section Cross References

    main.o(i.main) refers to board.o(i.board_Init) for board_Init
    main.o(i.main) refers to ap_demo.o(i.ap_demo) for ap_demo
    ap_demo.o(i.Gpio_swire_output) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    ap_demo.o(i.Gpio_swire_output) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.Gpio_swire_output) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    ap_demo.o(i.Gpio_swire_output) refers to tau_delay.o(i.delayUs) for delayUs
    ap_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) for hal_dsi_rx_ctrl_get_max_ret_size
    ap_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) for hal_dsi_rx_ctrl_send_ack_cmd
    ap_demo.o(i.ap_dcs_read) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_dcs_read) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_dcs_read) refers to app_tp_st_touch.o(i.ap_get_tp_calibration_status_01) for ap_get_tp_calibration_status_01
    ap_demo.o(i.ap_demo) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_I2C_init) for app_tp_I2C_init
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.open_mipi_rx) for open_mipi_rx
    ap_demo.o(i.ap_demo) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.init_mipi_tx) for init_mipi_tx
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_init) for app_tp_init
    ap_demo.o(i.ap_demo) refers to hal_timer.o(i.hal_timer_init) for hal_timer_init
    ap_demo.o(i.ap_demo) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.init_panel) for init_panel
    ap_demo.o(i.ap_demo) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    ap_demo.o(i.ap_demo) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.ap_demo) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_phone_clear_reset_on) for app_tp_phone_clear_reset_on
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_transfer_screen_start) for app_tp_transfer_screen_start
    ap_demo.o(i.ap_demo) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    ap_demo.o(i.ap_demo) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    ap_demo.o(i.ap_demo) refers to app_tp_st_touch.o(i.app_tp_calibration_exec) for app_tp_calibration_exec
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.tp_heartbeat_exec) for tp_heartbeat_exec
    ap_demo.o(i.ap_demo) refers to app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec) for ap_tp_st_touch_scan_point_record_event_exec
    ap_demo.o(i.ap_demo) refers to app_tp_transfer.o(i.app_tp_transfer_screen_int) for app_tp_transfer_screen_int
    ap_demo.o(i.ap_demo) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) for hal_dsi_rx_ctrl_dsc_async_handler
    ap_demo.o(i.ap_demo) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) for hal_dsi_tx_ctrl_stop
    ap_demo.o(i.ap_demo) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) for hal_dsi_tx_ctrl_deinit
    ap_demo.o(i.ap_demo) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) for hal_dsi_rx_ctrl_stop
    ap_demo.o(i.ap_demo) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) for hal_dsi_rx_ctrl_deinit
    ap_demo.o(i.ap_demo) refers to hal_system.o(i.hal_system_set_vcc) for hal_system_set_vcc
    ap_demo.o(i.ap_demo) refers to app_tp_for_custom_s8.o(.data) for tp_sleep_in
    ap_demo.o(i.ap_demo) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.soft_timer3_cb) for soft_timer3_cb
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.ap_reset_cb) for ap_reset_cb
    ap_demo.o(i.ap_get_reg_df) refers to memcpya.o(.text) for __aeabi_memcpy4
    ap_demo.o(i.ap_get_reg_df) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) for hal_dsi_tx_ctrl_set_ccm
    ap_demo.o(i.ap_get_reg_df) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_reset_cb) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_reset_cb) refers to hal_system.o(i.hal_system_set_pvd) for hal_system_set_pvd
    ap_demo.o(i.ap_reset_cb) refers to hal_system.o(i.hal_system_set_vcc) for hal_system_set_vcc
    ap_demo.o(i.ap_set_backlight_51) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_display_off) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_display_off) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_display_on) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) for hal_dsi_rx_ctrl_set_sw_tear_mode
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to ap_demo.o(i.Gpio_swire_output) for Gpio_swire_output
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_set_exit_sleep_mode) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_exit_sleep_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_exit_sleep_mode) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.ap_set_exit_sleep_mode) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) for hal_dsi_rx_ctrl_toggle_resolution
    ap_demo.o(i.ap_set_exit_sleep_mode) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_update_frame_rate) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex) for hal_dsi_rx_ctrl_set_tear_mode_ex
    ap_demo.o(i.ap_update_frame_rate) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_update_frame_rate) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.init_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) for hal_dsi_tx_ctrl_create_handle
    ap_demo.o(i.init_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    ap_demo.o(i.init_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) for hal_dsi_tx_ctrl_set_overwrite_rgb
    ap_demo.o(i.init_mipi_tx) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin) for hal_dsi_tx_ctrl_panel_reset_pin
    ap_demo.o(i.init_panel) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) for hal_dsi_tx_ctrl_enter_init_panel_mode
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) for hal_dsi_tx_ctrl_write_array_cmd
    ap_demo.o(i.init_panel) refers to tau_delay.o(i.delayUs) for delayUs
    ap_demo.o(i.init_panel) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    ap_demo.o(i.init_panel) refers to ap_demo.o(i.Gpio_swire_output) for Gpio_swire_output
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) for hal_dsi_tx_ctrl_exit_init_panel_mode
    ap_demo.o(i.init_panel) refers to ap_demo.o(.constdata) for .constdata
    ap_demo.o(i.open_mipi_rx) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) for hal_dsi_rx_ctrl_create_handle
    ap_demo.o(i.open_mipi_rx) refers to memcpya.o(.text) for __aeabi_memcpy4
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) for hal_dsi_rx_ctrl_pre_init_pps
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) for hal_dsi_rx_ctrl_set_cus_sync_line
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) for hal_dsi_rx_ctrl_set_cus_scld_filter
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) for hal_dsi_rx_ctrl_set_cus_esc_clk
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(.constdata) for .constdata
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(i.ap_dcs_read) for ap_dcs_read
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(i.pps_update_handle) for pps_update_handle
    ap_demo.o(i.pps_update_handle) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) for hal_dsi_rx_ctrl_toggle_resolution
    ap_demo.o(i.pps_update_handle) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.pps_update_handle) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.soft_timer3_cb) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    ap_demo.o(i.soft_timer3_cb) refers to app_tp_for_custom_s8.o(.data) for tp_sleep_count
    ap_demo.o(i.soft_timer3_cb) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.tp_heartbeat_exec) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    ap_demo.o(i.tp_heartbeat_exec) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.tp_heartbeat_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) for ap_tp_st_touch_software_reset
    ap_demo.o(i.tp_heartbeat_exec) refers to app_tp_transfer.o(.data) for s_screen_init_complate
    ap_demo.o(i.tp_heartbeat_exec) refers to ap_demo.o(.data) for .data
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_display_on) for ap_set_display_on
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_display_off) for ap_set_display_off
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_get_reg_df) for ap_get_reg_df
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_backlight_51) for ap_set_backlight_51
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_update_frame_rate) for ap_update_frame_rate
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_enter_sleep_mode) for ap_set_enter_sleep_mode
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_exit_sleep_mode) for ap_set_exit_sleep_mode
    ap_demo.o(.constdata) refers to app_tp_st_touch.o(i.ap_set_tp_calibration_04) for ap_set_tp_calibration_04
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_transfer.o(i.S20_Start_init) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.S20_Start_init) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_ctrl_eint) for hal_gpio_ctrl_eint
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_init_eint) for hal_gpio_init_eint
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_reg_eint_cb) for hal_gpio_reg_eint_cb
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_for_custom_s8.o(.data) for screen_reg_int_data
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(i.app_tp_screen_int_callback) for app_tp_screen_int_callback
    app_tp_transfer.o(i.S20_Start_init) refers to ap_demo.o(.data) for phone_start_flag
    app_tp_transfer.o(i.app_tp_I2C_init) refers to hal_i2c_slave.o(i.hal_i2c_s_init) for hal_i2c_s_init
    app_tp_transfer.o(i.app_tp_I2C_init) refers to hal_i2c_slave.o(i.hal_i2c_s_set_transfer) for hal_i2c_s_set_transfer
    app_tp_transfer.o(i.app_tp_I2C_init) refers to hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read) for hal_i2c_s_nonblocking_read
    app_tp_transfer.o(i.app_tp_I2C_init) refers to app_tp_transfer.o(i.app_tp_i2cs_callback) for app_tp_i2cs_callback
    app_tp_transfer.o(i.app_tp_I2C_init) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) for app_tp_phone_analysis_data
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(i.app_tp_s_read) for app_tp_s_read
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(i.app_tp_s_write) for app_tp_s_write
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.app_tp_init) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(i.app_tp_screen_init) for app_tp_screen_init
    app_tp_transfer.o(i.app_tp_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    app_tp_transfer.o(i.app_tp_init) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_master.o(i.hal_i2c_m_dma_init) for hal_i2c_m_dma_init
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_for_custom_s8.o(.data) for g_phone_output_int_pad
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.app_tp_m_read) refers to hal_i2c_master.o(i.hal_i2c_m_dma_read) for hal_i2c_m_dma_read
    app_tp_transfer.o(i.app_tp_m_transfer_complate) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.app_tp_m_write) refers to hal_i2c_master.o(i.hal_i2c_m_dma_write) for hal_i2c_m_dma_write
    app_tp_transfer.o(i.app_tp_phone_clear_reset_on) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_phone_reset_on) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_s_read) refers to hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read) for hal_i2c_s_nonblocking_read
    app_tp_transfer.o(i.app_tp_s_transfer_complate) refers to hal_i2c_slave.o(i.hal_i2c_s_write_complate) for hal_i2c_s_write_complate
    app_tp_transfer.o(i.app_tp_s_transfer_complate) refers to hal_i2c_slave.o(i.hal_i2c_s_read_complate) for hal_i2c_s_read_complate
    app_tp_transfer.o(i.app_tp_s_write) refers to hal_i2c_slave.o(i.hal_i2c_s_dma_write) for hal_i2c_s_dma_write
    app_tp_transfer.o(i.app_tp_screen_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    app_tp_transfer.o(i.app_tp_screen_init) refers to tau_delay.o(i.delayUs) for delayUs
    app_tp_transfer.o(i.app_tp_screen_init) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_transfer.o(i.app_tp_screen_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_rst_pad
    app_tp_transfer.o(i.app_tp_screen_int_callback) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to hal_spi_master.o(i.hal_spi_m_clear_rxfifo) for hal_spi_m_clear_rxfifo
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(i.S20_Start_init) for S20_Start_init
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_for_custom_s8.o(.constdata) for screen_reg_start_data_size
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to ap_demo.o(.data) for phone_start_flag
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_transfer_screen_const) for app_tp_transfer_screen_const
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_F3) for ap_tp_st_touch_error_handler_F3
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_FF) for ap_tp_st_touch_error_handler_FF
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event) for ap_tp_st_touch_scan_point_record_event
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to tau_delay.o(i.delayUs) for delayUs
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) for app_tp_screen_analysis_int
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to tau_log.o(i.LOG_printf) for LOG_printf
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(.data) for screen_reg_int_data
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.app_tp_transfer_screen_start) refers to app_tp_transfer.o(i.app_tp_transfer_screen_const) for app_tp_transfer_screen_const
    app_tp_transfer.o(i.app_tp_transfer_screen_start) refers to app_tp_transfer.o(.data) for .data
    app_tp_st_touch.o(i.CRC16_2) refers to app_tp_st_touch.o(.constdata) for .constdata
    app_tp_st_touch.o(i.ap_get_tp_calibration_status_01) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) for hal_dsi_rx_ctrl_send_ack_cmd
    app_tp_st_touch.o(i.ap_get_tp_calibration_status_01) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.ap_set_tp_calibration_04) refers to memseta.o(.text) for __aeabi_memclr4
    app_tp_st_touch.o(i.ap_set_tp_calibration_04) refers to printfa.o(i.__0printf) for __2printf
    app_tp_st_touch.o(i.ap_set_tp_calibration_04) refers to app_tp_st_touch.o(i.CRC16_2) for CRC16_2
    app_tp_st_touch.o(i.ap_set_tp_calibration_04) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.ap_tp_st_touch_calibration) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_st_touch.o(i.ap_tp_st_touch_calibration) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_st_touch.o(i.ap_tp_st_touch_calibration) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_calibration) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_F3) refers to app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) for ap_tp_st_touch_software_reset
    app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_FF) refers to app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) for ap_tp_st_touch_software_reset
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to memseta.o(.text) for __aeabi_memclr4
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to tau_log.o(i.LOG_printf) for LOG_printf
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event) for ap_tp_st_touch_simulate_finger_release_event
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init) for ap_tp_st_touch_scan_point_init
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_rst_pad
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init) refers to app_tp_st_touch.o(.bss) for .bss
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event) refers to app_tp_st_touch.o(.bss) for .bss
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec) refers to printfa.o(i.__0printf) for __2printf
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event) for ap_tp_st_touch_simulate_finger_release_event
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init) for ap_tp_st_touch_scan_point_init
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec) refers to app_tp_st_touch.o(.bss) for .bss
    app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event) refers to app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) for app_tp_screen_analysis_int
    app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to tau_log.o(i.LOG_printf) for LOG_printf
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event) for ap_tp_st_touch_simulate_finger_release_event
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init) for ap_tp_st_touch_scan_point_init
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_calibration) for ap_tp_st_touch_calibration
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) for ap_tp_st_touch_get_calibration_success_mark
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to tau_log.o(i.LOG_printf) for LOG_printf
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to app_tp_st_touch.o(.data) for .data
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_init) for hal_system_init
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_enable_systick) for hal_system_enable_systick
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_init_console) for hal_system_init_console
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_set_phy_calibration) for hal_system_set_phy_calibration
    startup_armcm0.o(RESET) refers to startup_armcm0.o(STACK) for __initial_sp
    startup_armcm0.o(RESET) refers to startup_armcm0.o(.text) for Reset_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.HardFault_Handler) for HardFault_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SysTick_Handler) for SysTick_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.VIDC_IRQn_Handler) for VIDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.LCDC_IRQn_Handler) for LCDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.MIPI_RX_IRQn_Handler) for MIPI_RX_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.MIPI_TX_IRQn_Handler) for MIPI_TX_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.MEMC_IRQn_Handler) for MEMC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.VPRE_IRQn_Handler) for VPRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.FLSCTRL_IRQn_Handler) for FLSCTRL_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.DMA_IRQn_Handler) for DMA_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER0_IRQn_Handler) for TIMER0_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER1_IRQn_Handler) for TIMER1_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER2_IRQn_Handler) for TIMER2_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER3_IRQn_Handler) for TIMER3_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.WDG_IRQn_Handler) for WDG_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.UART_IRQn_Handler) for UART_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.I2C0_IRQn_Handler) for I2C0_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.I2C1_IRQn_Handler) for I2C1_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SPIS_IRQn_Handler) for SPIS_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SPIM_IRQn_Handler) for SPIM_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.ADC_IRQn_Handler) for ADC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.PWMDET_IRQn_Handler) for PWMDET_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SWIRE_IRQn_Handler) for SWIRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.AP_NRESET_IRQn_Handler) for AP_NRESET_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT0_IRQn_Handler) for EXTI_INT0_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT1_IRQn_Handler) for EXTI_INT1_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT2_IRQn_Handler) for EXTI_INT2_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT3_IRQn_Handler) for EXTI_INT3_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT4_IRQn_Handler) for EXTI_INT4_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT5_IRQn_Handler) for EXTI_INT5_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT6_IRQn_Handler) for EXTI_INT6_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT7_IRQn_Handler) for EXTI_INT7_IRQn_Handler
    startup_armcm0.o(.text) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to drv_vidc.o(i.drv_vidc_set_module_enable) for drv_vidc_set_module_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) for hal_internal_vsync_get_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) for dcs_packet_get_fifo_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) for dcs_packet_free_fifo_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg) for drv_dsi_rx_set_ddi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_crgu.o(i.drv_crgu_set_rxbr_src) for drv_crgu_set_rxbr_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_crgu.o(i.drv_crgu_set_rxbr_div) for drv_crgu_set_rxbr_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg) for drv_dsi_rx_set_ipi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_gen_a_tear_signal) for drv_memc_gen_a_tear_signal
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size) for drv_dsi_rx_get_max_ret_size
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_rxbr_src) for drv_crgu_set_rxbr_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_rxbr_div) for drv_crgu_set_rxbr_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_dsco_src) for drv_crgu_set_dsco_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_dsco_src_div) for drv_crgu_set_dsco_src_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_dsc_core_div) for drv_crgu_set_dsc_core_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_vidc_src) for drv_crgu_set_vidc_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_fb_src) for drv_crgu_set_fb_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to drv_crgu.o(i.drv_crgu_set_fb_div) for drv_crgu_set_fb_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) for hal_dsi_rx_ctrl_init_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_rx) for hal_internal_vsync_init_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) for hal_dsi_rx_ctrl_init_dsi_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) for hal_dsi_rx_ctrl_init_rxbr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps) for drv_dsc_dec_set_u8_pps
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) for hal_dsi_rx_ctrl_init_vidc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) for hal_dsi_rx_ctrl_init_memc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_chip_info.o(i.drv_chip_rx_init_done) for drv_chip_rx_init_done
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_vidc_src) for drv_crgu_set_vidc_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_fb_src) for drv_crgu_set_fb_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_fb_div) for drv_crgu_set_fb_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) for hal_dsi_rx_ctrl_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg) for drv_dsi_rx_set_ctrl_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) for drv_dsi_rx_set_up_phy
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap) for drv_dsi_rx_set_lane_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_inten) for drv_dsi_rx_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt) for drv_dsi_rx_set_resp_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_mode) for drv_memc_set_ltpo_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_fs_en_conditions) for drv_memc_set_fs_en_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_lcdc_st_conditions) for drv_memc_set_lcdc_st_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_vidc_sync_cnt) for drv_memc_set_vidc_sync_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_double_buffer) for drv_memc_set_double_buffer
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_active_height) for drv_memc_set_active_height
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_inten) for drv_memc_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_color_format) for drv_rxbr_set_color_format
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th) for drv_rxbr_set_ltpo_drop_th
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_cfg) for drv_rxbr_set_usr_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_col) for drv_rxbr_set_usr_col
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_row) for drv_rxbr_set_usr_row
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg) for drv_rxbr_hline_rcv_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) for hal_internal_vsync_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_src_parameter) for drv_vidc_set_src_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pentile_swap) for drv_vidc_set_pentile_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_dst_parameter) for drv_vidc_set_dst_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_init_module_enable) for drv_vidc_init_module_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_rotation) for drv_vidc_set_rotation
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_init_get_scld_filter_h) for drv_param_init_get_scld_filter_h
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_init_get_scld_filter_v) for drv_param_init_get_scld_filter_v
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef0) for drv_vidc_set_scld_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef1) for drv_vidc_set_scld_hcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef0) for drv_vidc_set_scld_vcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef1) for drv_vidc_set_scld_vcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_p2r_hinitr) for drv_vidc_set_p2r_hinitr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_p2r_hinitb) for drv_vidc_set_p2r_hinitb
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_p2r_filter_init) for drv_param_p2r_filter_init
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_p2r_hcoef0) for drv_vidc_set_p2r_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_mirror) for drv_vidc_set_mirror
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pu_ctrl) for drv_vidc_set_pu_ctrl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter) for drv_dsc_dec_convert_pps_rc_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header) for drv_rxbr_set_ack_pkt_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) for hal_internal_vsync_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef0) for drv_vidc_set_scld_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef1) for drv_vidc_set_scld_hcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef0) for drv_vidc_set_scld_vcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef1) for drv_vidc_set_scld_vcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_param_init.o(i.drv_param_init_set_scld_filter) for drv_param_init_set_scld_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) for hal_internal_vsync_set_sync_line
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg) for drv_rxbr_hline_rcv0_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_dcs_direct_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode) for hal_internal_vsync_set_dcs_direct_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) refers to drv_rxbr.o(i.drv_rxbr_set_cmd_filter) for drv_rxbr_set_cmd_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) for drv_dsi_rx_calc_ipi_tx_delay
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg) for drv_dsi_rx_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format) refers to drv_vidc.o(i.drv_vidc_update_src_format) for drv_vidc_update_src_format
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format) refers to drv_vidc.o(i.drv_vidc_set_pentile_swap) for drv_vidc_set_pentile_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dflti.o(.text) for __aeabi_i2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dmul.o(.text) for __aeabi_dmul
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to ddiv.o(.text) for __aeabi_ddiv
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) for hal_dsi_rx_ctrl_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_src) for drv_crgu_set_rxbr_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_div) for drv_crgu_set_rxbr_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_dsco_src) for drv_crgu_set_dsco_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_dsco_src_div) for drv_crgu_set_dsco_src_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_dsc_core_div) for drv_crgu_set_dsc_core_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_te_waveform) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_te_waveform) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_dsi_rx.o(i.drv_dsi_rx_power_up) for drv_dsi_rx_power_up
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg) for drv_rxbr_hline_rcv0_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) for hal_internal_sync_input_resolution_change
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fscalb.o(.text) for __ARM_scalbnf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fflti.o(.text) for __aeabi_i2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to ffixi.o(.text) for __aeabi_f2iz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk) for drv_dsi_tx_set_video_chunk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing) for drv_dsi_tx_set_video_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to drv_phy_common.o(i.drv_phy_get_rate_para) for drv_phy_get_rate_para
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to fadd.o(.text) for __aeabi_fsub
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to ffixui.o(.text) for __aeabi_f2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) for hal_lcdc_config_upscaler
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to drv_lcdc.o(i.drv_lcdc_config_src_parameter) for drv_lcdc_config_src_parameter
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_ulps_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) for drv_dsi_tx_phy_ulps_enter
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_ulps_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) for drv_dsi_tx_phy_ulps_exit
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) for hal_dsi_tx_ctrl_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_tx) for hal_internal_vsync_init_tx
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate) for hal_dsi_tx_config_params_for_lane_rate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) for hal_dsi_tx_count_lane_rate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) for hal_dsi_tx_init_phy_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) for drv_dsi_tx_phy_test_setup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) for hal_lcdc_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) for hal_lcdc_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) for hal_dsi_tx_init_dpi_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) for hal_dsi_tx_init_data_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) for hal_dsi_tx_init_remains
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt) for hal_dsi_tx_init_interrupt
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready) for drv_dsi_tx_phy_status_ready
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload) for drv_dsi_tx_command_get_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) refers to drv_param_init.o(i.drv_param_init_set_ccm) for drv_param_init_set_ccm
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_pq_filter) refers to drv_lcdc.o(i.drv_lcdc_config_scale_up_coef) for drv_lcdc_config_scale_up_coef
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_pq_filter) refers to drv_param_init.o(i.drv_param_init_set_sclu_filter) for drv_param_init_set_sclu_filter
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness) refers to drv_lcdc.o(i.drv_lcdc_config_endianness) for drv_lcdc_config_endianness
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_lp_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd) for drv_dsi_tx_video_mode_set_lp_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb) for drv_lcdc_config_overwrite_rgb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp) refers to drv_lcdc.o(i.drv_lcdc_config_partial_display_enable) for drv_lcdc_config_partial_display_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area) refers to drv_lcdc.o(i.drv_lcdc_config_partial_display_area) for drv_lcdc_config_partial_display_area
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_vpg) for drv_dsi_tx_set_vpg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_enable_shadow_reg) for drv_lcdc_enable_shadow_reg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_set_video_hw_mode) for drv_lcdc_set_video_hw_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_start) for drv_lcdc_start
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_lcdc.o(i.drv_lcdc_start) for drv_lcdc_start
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size) for drv_dsi_tx_edpi_cmd_size
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) for hal_dsi_tx_init_video_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode) for drv_dsi_tx_dpi_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity) for drv_dsi_tx_dpi_polarity
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time) for drv_dsi_tx_dpi_lpcmd_time
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_int) for drv_dsi_tx_config_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode) for drv_dsi_tx_phy_lane_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg) for drv_dsi_tx_phy_time_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_response_mode) for drv_dsi_tx_response_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div) for drv_dsi_tx_set_time_out_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg) for drv_dsi_tx_timeout_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp) for drv_dsi_tx_phy_clock_lane_auto_lp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg) for drv_dsi_tx_video_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack) for drv_dsi_tx_set_bta_ack
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd) for drv_dsi_tx_video_mode_set_lp_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_disable_hact_cmd) for drv_dsi_tx_video_mode_disable_hact_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) for hal_dsi_tx_calc_video_chunks
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_header) for drv_dsi_tx_command_header
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) refers to drv_param_init.o(i.drv_param_init_get_ccm) for drv_param_init_get_ccm
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) refers to drv_lcdc.o(i.drv_lcdc_config_ccm) for drv_lcdc_config_ccm
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_disp_mode) for drv_lcdc_config_disp_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_edpi_mode) for drv_lcdc_config_edpi_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_endianness) for drv_lcdc_config_endianness
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_thresh) for drv_lcdc_config_thresh
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_dpi_polarity) for drv_lcdc_config_dpi_polarity
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_src_parameter) for drv_lcdc_config_src_parameter
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area) for hal_dsi_tx_ctrl_set_partial_disp_area
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp) for hal_dsi_tx_ctrl_set_partial_disp
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_lcdc.o(i.drv_lcdc_config_scale_up_step) for drv_lcdc_config_scale_up_step
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_param_init.o(i.drv_param_init_get_sclu_filter) for drv_param_init_get_sclu_filter
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_lcdc.o(i.drv_lcdc_config_scale_up_coef) for drv_lcdc_config_scale_up_coef
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) for hal_lcdc_config_upscaler
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) for hal_lcdc_config_ccm
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile) for hal_lcdc_config_rgb_to_pentile
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) for hal_lcdc_config_remains
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) for hal_lcdc_init_interrupt
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dpi_pre_div) for drv_crgu_set_dpi_pre_div
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dpi_pre_src) for drv_crgu_set_dpi_pre_src
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dpi_mux_src) for drv_crgu_set_dpi_mux_src
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_lcdc.o(i.drv_lcdc_config_dpi_timing) for drv_lcdc_config_dpi_timing
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to cfrcmple.o(.text) for __aeabi_cfrcmple
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ffixi.o(.text) for __aeabi_f2iz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_lcdc_div) for drv_crgu_set_lcdc_div
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_lcdc_src) for drv_crgu_set_lcdc_src
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to drv_lcdc.o(i.drv_lcdc_ctrl_flow) for drv_lcdc_ctrl_flow
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to drv_lcdc.o(i.drv_lcdc_config_int) for drv_lcdc_config_int
    hal_gpio.o(i.hal_gpio_ctrl_eint) refers to drv_gpio.o(i.drv_gpio_set_int) for drv_gpio_set_int
    hal_gpio.o(i.hal_gpio_ctrl_eint) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_get_input_data) refers to drv_gpio.o(i.drv_gpio_get_input_data) for drv_gpio_get_input_data
    hal_gpio.o(i.hal_gpio_get_int_type) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to drv_gpio.o(i.drv_gpio_get_pull_state) for drv_gpio_get_pull_state
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_eint) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group) for drv_sys_cfg_sel_gpio_group
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig) for drv_sys_cfg_sel_int_trig
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_init_eint) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_input) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_input) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_input) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_init_output) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_reg_eint_cb) refers to drv_gpio.o(i.drv_gpio_register_callback) for drv_gpio_register_callback
    hal_gpio.o(i.hal_gpio_reg_eint_cb) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_gpio.o(i.drv_gpio_register_ap_reset_callback) for drv_gpio_register_ap_reset_callback
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) for drv_sys_cfg_sel_ap_rst_trig
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to drv_gpio.o(i.drv_gpio_set_driving_strength) for drv_gpio_set_driving_strength
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode3) for drv_gpio_set_mode3
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode2) for drv_gpio_set_mode2
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode1) for drv_gpio_set_mode1
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode0) for drv_gpio_set_mode0
    hal_gpio.o(i.hal_gpio_set_mode) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_output_data) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to drv_gpio.o(i.drv_gpio_set_pull_state) for drv_gpio_set_pull_state
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to drv_gpio.o(i.drv_gpio_set_schmitt_trigger) for drv_gpio_set_schmitt_trigger
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to drv_gpio.o(i.drv_gpio_set_slew_rate) for drv_gpio_set_slew_rate
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to hal_gpio.o(.constdata) for .constdata
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_master.o(i.drv_i2c_master_init) for drv_i2c_master_init
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_master.o(i.drv_i2c_m_set_callback) for drv_i2c_m_set_callback
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_master.o(i.drv_i2c_m_enable_intr) for drv_i2c_m_enable_intr
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_dma.o(i.drv_i2c_dma_init) for drv_i2c_dma_init
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_dma.o(i.drv_i2c_enable_rx_dma) for drv_i2c_enable_rx_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_dma.o(i.drv_i2c_enable_tx_dma) for drv_i2c_enable_tx_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to hal_i2c_master.o(i.hal_i2c_master_irq_callback) for hal_i2c_master_irq_callback
    hal_i2c_master.o(i.hal_i2c_m_dma_read) refers to drv_i2c_dma.o(i.drv_i2c_master_read_dma) for drv_i2c_master_read_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_read) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_master.o(i.hal_i2c_m_dma_write) refers to drv_i2c_dma.o(i.drv_i2c_master_write_dma) for drv_i2c_master_write_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_write) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_master.o(i.hal_i2c_m_set_high_impedance) refers to drv_i2c_master.o(i.drv_i2c_m_enable) for drv_i2c_m_enable
    hal_i2c_master.o(i.hal_i2c_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_master.o(i.hal_i2c_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_i2c_master.o(i.hal_i2c_m_transfer_complate) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_master.o(i.hal_i2c_master_irq_callback) refers to drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit) for drv_i2c_m_clear_it_pending_bit
    hal_i2c_master.o(i.hal_i2c_master_irq_callback) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to drv_i2c_dma.o(i.drv_i2c_slave_write_dma) for drv_i2c_slave_write_dma
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_get_tx_byte_num) refers to drv_i2c_slave.o(i.drv_i2c_s_get_tx_byte_num) for drv_i2c_s_get_tx_byte_num
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c_slave_init) for drv_i2c_slave_init
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c_s_set_callback) for drv_i2c_s_set_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c_s_enable_intr) for drv_i2c_s_enable_intr
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_dma.o(i.drv_i2c_dma_init) for drv_i2c_dma_init
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) for drv_i2c_set_dma_irq_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_dma.o(i.drv_i2c_enable_tx_dma) for drv_i2c_enable_tx_dma
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) for hal_i2c_slave_irq_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback) for hal_i2c_s_dma_user_callback
    hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_complate) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_complate_clear) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_data) refers to drv_i2c_slave.o(i.drv_i2c_s_read_data) for drv_i2c_s_read_data
    hal_i2c_slave.o(i.hal_i2c_s_rxfifo_notempty) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    hal_i2c_slave.o(i.hal_i2c_s_set_dma_tx_cycle) refers to drv_dma.o(i.drv_dma_enable_cycle) for drv_dma_enable_cycle
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to drv_i2c_slave.o(i.drv_i2c_s_enable) for drv_i2c_s_enable
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_i2c_slave.o(i.hal_i2c_s_set_transfer) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_write_complate) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_write_data) refers to drv_i2c_slave.o(i.drv_i2c_s_write_data) for drv_i2c_s_write_data
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit) for drv_i2c_s_clear_it_pending_bit
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(i.drv_i2c_s_write_data) for drv_i2c_s_write_data
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(.data) for tx_byte_num
    hal_spi_master.o(i.hal_spi_m_callback) refers to drv_spi_dma.o(i.drv_spi_abort_dma) for drv_spi_abort_dma
    hal_spi_master.o(i.hal_spi_m_callback) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_clear_rxfifo) refers to drv_spi_master.o(i.drv_spi_m_read_data) for drv_spi_m_read_data
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to hal_spi_master.o(i.hal_spi_m_gpio_init) for hal_spi_m_gpio_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_master.o(i.drv_spi_master_init) for drv_spi_master_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_dma_init) for drv_spi_dma_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_dma_ch6_init) for drv_spi_dma_ch6_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) for drv_spi_set_dma_irq_callback
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) for drv_spi_set_dma_ch6_irq_callback
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req) for drv_sys_cfg_set_dma_rx_req
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_master.o(i.drv_spi_m_enable_rx_dma) for drv_spi_m_enable_rx_dma
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to hal_spi_master.o(i.hal_spi_m_callback) for hal_spi_m_callback
    hal_spi_master.o(i.hal_spi_m_dma_read) refers to drv_spi_dma.o(i.drv_spim_dma_read) for drv_spim_dma_read
    hal_spi_master.o(i.hal_spi_m_dma_read) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_dma_write) refers to drv_spi_dma.o(i.drv_spim_dma_write) for drv_spim_dma_write
    hal_spi_master.o(i.hal_spi_m_dma_write) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_get_transfer_complate) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_gpio_init) refers to drv_spi_master.o(i.drv_spi_m_gpio_init) for drv_spi_m_gpio_init
    hal_spi_master.o(i.hal_spi_m_read_rxfifo) refers to drv_spi_master.o(i.drv_spi_m_read_data) for drv_spi_m_read_data
    hal_spi_master.o(i.hal_spi_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_spi_master.o(i.hal_spi_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    hal_spi_master.o(i.hal_spi_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_system.o(i.hal_system_deep_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode) for drv_pwr_enter_deep_sleep_mode
    hal_system.o(i.hal_system_disable_systick) refers to drv_common.o(i.drv_common_disable_systick) for drv_common_disable_systick
    hal_system.o(i.hal_system_enable_systick) refers to drv_common.o(i.drv_common_enable_systick) for drv_common_enable_systick
    hal_system.o(i.hal_system_flash_read) refers to norflash.o(i.norflash_init) for norflash_init
    hal_system.o(i.hal_system_flash_read) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    hal_system.o(i.hal_system_flash_read) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_system.o(i.hal_system_flash_read) refers to norflash.o(i.norflash_dual_read) for norflash_dual_read
    hal_system.o(i.hal_system_flash_write) refers to norflash.o(i.norflash_init) for norflash_init
    hal_system.o(i.hal_system_flash_write) refers to norflash.o(i.norflash_erase_block) for norflash_erase_block
    hal_system.o(i.hal_system_flash_write) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_system.o(i.hal_system_flash_write) refers to norflash.o(i.norflash_write) for norflash_write
    hal_system.o(i.hal_system_get_tick) refers to drv_common.o(i.drv_common_get_tick) for drv_common_get_tick
    hal_system.o(i.hal_system_idle_mode) refers to drv_common.o(i.drv_common_idle_mode) for drv_common_idle_mode
    hal_system.o(i.hal_system_init) refers to drv_pwr.o(i.drv_pwr_set_system_clk_src) for drv_pwr_set_system_clk_src
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_set_ahb_src) for drv_crgu_set_ahb_src
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_set_ahb_pre_div) for drv_crgu_set_ahb_pre_div
    hal_system.o(i.hal_system_init) refers to irq_redirect .o(i.handle_init) for handle_init
    hal_system.o(i.hal_system_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int) for drv_sys_cfg_clear_all_int
    hal_system.o(i.hal_system_init) refers to drv_common.o(i.drv_common_system_init) for drv_common_system_init
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_system.o(i.hal_system_init) refers to drv_pwr.o(i.drv_pwr_set_pvd_mode) for drv_pwr_set_pvd_mode
    hal_system.o(i.hal_system_init) refers to drv_common.o(.data) for g_system_clock
    hal_system.o(i.hal_system_init_console) refers to hal_uart.o(i.hal_uart_init) for hal_uart_init
    hal_system.o(i.hal_system_register_systick_cb) refers to drv_common.o(i.drv_common_systick_register_cb) for drv_common_systick_register_cb
    hal_system.o(i.hal_system_set_phy_calibration) refers to drv_phy_common.o(i.drv_phy_enable_calibration) for drv_phy_enable_calibration
    hal_system.o(i.hal_system_set_pvd) refers to drv_pwr.o(i.drv_pwr_set_pvd_mode) for drv_pwr_set_pvd_mode
    hal_system.o(i.hal_system_set_vcc) refers to drv_pwr.o(i.drv_pwr_set_cp_mode) for drv_pwr_set_cp_mode
    hal_system.o(i.hal_system_share_flash_mode) refers to drv_fls.o(i.drv_fls_gpio_connect) for drv_fls_gpio_connect
    hal_system.o(i.hal_system_share_flash_mode) refers to drv_fls.o(i.drv_fls_gpio_disconnect) for drv_fls_gpio_disconnect
    hal_system.o(i.hal_system_sleep_mode) refers to drv_crgu.o(i.drv_crgu_config_clocks) for drv_crgu_config_clocks
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_set_repeat) for drv_timer_set_repeat
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_timer.o(i.hal_timer_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_timer.o(i.hal_timer_get_status) refers to drv_timer.o(i.drv_timer_get_current_count) for drv_timer_get_current_count
    hal_timer.o(i.hal_timer_get_status) refers to drv_timer.o(i.drv_timer_get_match) for drv_timer_get_match
    hal_timer.o(i.hal_timer_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_timer.o(i.hal_timer_init) refers to drv_timer.o(i.drv_timer_set_prescaler) for drv_timer_set_prescaler
    hal_timer.o(i.hal_timer_set_repeat) refers to drv_timer.o(i.drv_timer_set_repeat) for drv_timer_set_repeat
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_get_prescaler) for drv_timer_get_prescaler
    hal_timer.o(i.hal_timer_start) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_match) for drv_timer_set_match
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_current_count) for drv_timer_set_current_count
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_start) refers to drv_common.o(.data) for g_system_clock
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_match) for drv_timer_set_match
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_current_count) for drv_timer_set_current_count
    tau_delay.o(i.delayMs) refers to tau_delay.o(i.delayUs) for delayUs
    tau_log.o(i.LOG_printf) refers to printfa.o(i.__0vsprintf) for vsprintf
    tau_log.o(i.LOG_printf) refers to printfa.o(i.__0printf) for __2printf
    tau_log.o(i.LOG_printf) refers to tau_log.o(.bss) for .bss
    tau_log.o(i.fgetc) refers to hal_uart.o(i.hal_uart_receive_blocking) for hal_uart_receive_blocking
    tau_log.o(i.fputc) refers to hal_uart.o(i.hal_uart_transmit_blocking) for hal_uart_transmit_blocking
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to app_tp_for_custom_s8.o(.data) for .data
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to app_tp_for_custom_s8.o(.constdata) for .constdata
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to app_tp_transfer.o(i.app_tp_screen_init) for app_tp_screen_init
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to app_tp_for_custom_s8.o(.data) for .data
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to uidiv.o(.text) for __aeabi_uidivmod
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to app_tp_for_custom_s8.o(.data) for .data
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_1
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_2
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_3
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_4
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_5
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_6
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_7
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_point_data
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_point_back
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_coord_data
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_coord_back
    hal_uart.o(i.hal_uart_deinit) refers to drv_dma.o(i.drv_dma_deinit) for drv_dma_deinit
    hal_uart.o(i.hal_uart_deinit) refers to drv_uart.o(i.UART_Deinit) for UART_Deinit
    hal_uart.o(i.hal_uart_dmacallback) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_uart.o(i.hal_uart_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_uart.o(i.hal_uart_init) refers to drv_uart.o(i.UART_init) for UART_init
    hal_uart.o(i.hal_uart_init) refers to drv_common.o(.data) for g_system_clock
    hal_uart.o(i.hal_uart_init) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_receive_blocking) refers to drv_uart.o(i.UART_ReadBlocking) for UART_ReadBlocking
    hal_uart.o(i.hal_uart_receive_dma) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    hal_uart.o(i.hal_uart_receive_dma) refers to drv_uart_dma.o(i.UART_TransferCreateHandleDMA) for UART_TransferCreateHandleDMA
    hal_uart.o(i.hal_uart_receive_dma) refers to drv_uart_dma.o(i.UART_TransferReceiveDMA) for UART_TransferReceiveDMA
    hal_uart.o(i.hal_uart_receive_dma) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_receive_dma) refers to hal_uart.o(i.hal_uart_dmacallback) for hal_uart_dmacallback
    hal_uart.o(i.hal_uart_transmit_blocking) refers to drv_uart.o(i.UART_WriteBlocking) for UART_WriteBlocking
    hal_uart.o(i.hal_uart_transmit_dma) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    hal_uart.o(i.hal_uart_transmit_dma) refers to drv_uart_dma.o(i.UART_TransferCreateHandleDMA) for UART_TransferCreateHandleDMA
    hal_uart.o(i.hal_uart_transmit_dma) refers to drv_uart_dma.o(i.UART_TransferSendDMA) for UART_TransferSendDMA
    hal_uart.o(i.hal_uart_transmit_dma) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_transmit_dma) refers to hal_uart.o(i.hal_uart_dmacallback) for hal_uart_dmacallback
    norflash.o(i.app_fls_ctrl_Handler) refers to drv_fls.o(i.fls_clr_interrupt_flag) for fls_clr_interrupt_flag
    norflash.o(i.app_fls_ctrl_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    norflash.o(i.app_fls_ctrl_Handler) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_best_cfg_init) refers to drv_fls.o(i.fls_spi_init) for fls_spi_init
    norflash.o(i.norflash_best_cfg_init) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_check_id) refers to norflash.o(i.norflash_read_id) for norflash_read_id
    norflash.o(i.norflash_check_id) refers to tau_delay.o(i.delayUs) for delayUs
    norflash.o(i.norflash_check_id) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dma_callback) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dma_read) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_transfer_create_handle_dma) for fls_transfer_create_handle_dma
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_dma_read_prepare) for fls_dma_read_prepare
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_transfer_dma) for fls_transfer_dma
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    norflash.o(i.norflash_dma_read) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dma_read) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_dma_read) refers to norflash.o(i.norflash_dma_callback) for norflash_dma_callback
    norflash.o(i.norflash_dma_write) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_transfer_create_handle_dma) for fls_transfer_create_handle_dma
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_switch_fls_spi) for norflash_switch_fls_spi
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_dma_write_prepare) for fls_dma_write_prepare
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_transfer_dma) for fls_transfer_dma
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    norflash.o(i.norflash_dma_write) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_dma_write) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_dma_callback) for norflash_dma_callback
    norflash.o(i.norflash_dma_write) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dual_read) refers to drv_fls.o(i.fls_ddat_enable) for fls_ddat_enable
    norflash.o(i.norflash_dual_read) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_dual_read) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_switch_fls_spi) for norflash_switch_fls_spi
    norflash.o(i.norflash_dual_write) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_dual_write) refers to drv_fls.o(i.fls_ddat_enable) for fls_ddat_enable
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_en4b) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_read_config_reg) for norflash_read_config_reg
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_en_quad) refers to norflash.o(i.norflash_en_quad_check) for norflash_en_quad_check
    norflash.o(i.norflash_en_quad) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_en_quad) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_en_quad) refers to drv_fls.o(i.fls_busy_pending) for fls_busy_pending
    norflash.o(i.norflash_en_quad) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(i.norflash_get_dual_hstatus) for norflash_get_dual_hstatus
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(i.norflash_get_hstatus) for norflash_get_hstatus
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_erase_block) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_erase_block) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_erase_block) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_erase_block) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_erase_chip) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_erase_chip) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_erase_chip) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_erase_sector) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_erase_sector) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_erase_sector) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_erase_sector) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_ex4b) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_read_config_reg) for norflash_read_config_reg
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_exit_quad) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_exit_quad) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_exit_quad) refers to norflash.o(i.norflash_en_quad_check) for norflash_en_quad_check
    norflash.o(i.norflash_exit_quad) refers to drv_fls.o(i.fls_busy_pending) for fls_busy_pending
    norflash.o(i.norflash_exit_quad) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_get_dual_hstatus) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_get_dual_hstatus) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_get_dual_hstatus) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_get_hstatus) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_get_hstatus) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_get_hstatus) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_get_status) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_get_status) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_get_status) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_get_default_spi_config) for fls_get_default_spi_config
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_get_default_fls_config) for fls_get_default_fls_config
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_get_default_tuning) for fls_get_default_tuning
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_init) for fls_init
    norflash.o(i.norflash_init) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_init) refers to drv_fls.o(.data) for g_fls_tuning
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_qdat_enable) for fls_qdat_enable
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_qadr_enable) for fls_qadr_enable
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_qcmd_enable) for fls_qcmd_enable
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_switch_fls_spi) for norflash_switch_fls_spi
    norflash.o(i.norflash_quad_write) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_quad_write) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_read) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_read_config_reg) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_read_id) refers to drv_fls.o(i.fls_read_cmd) for fls_read_cmd
    norflash.o(i.norflash_set_best_cfg) refers to memseta.o(.text) for __aeabi_memclr4
    norflash.o(i.norflash_set_best_read_cfg) refers to norflash.o(i.norflash_en_quad) for norflash_en_quad
    norflash.o(i.norflash_set_best_read_cfg) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_set_best_read_cfg) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_set_best_write_cfg) refers to norflash.o(i.norflash_en_quad) for norflash_en_quad
    norflash.o(i.norflash_set_best_write_cfg) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_set_best_write_cfg) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_ddat_enable) for fls_ddat_enable
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_qdat_enable) for fls_qdat_enable
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_qadr_enable) for fls_qadr_enable
    norflash.o(i.norflash_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_write) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_write_disable) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_write_disable) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write_disable) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_write_disable) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_write_enable) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_write_enable) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write_enable) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_write_enable) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_big_end_enable) for norflash_big_end_enable
    norflash.o(i.norflash_write_endian_scr) refers to drv_fls.o(i.fls_en_scr) for fls_en_scr
    norflash.o(i.norflash_write_endian_scr) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_big_end_clear) for norflash_big_end_clear
    norflash.o(i.norflash_write_endian_scr) refers to drv_fls.o(i.fls_scr_clear) for fls_scr_clear
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    drv_common.o(i.app_HardFault_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_common.o(i.app_SysTick_Handler) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_enable_systick) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_common.o(i.drv_common_enable_systick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_get_tick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_system_init) refers to drv_chip_info.o(i.drv_chip_info_init) for drv_chip_info_init
    drv_common.o(i.drv_common_systick_register_cb) refers to drv_common.o(.data) for .data
    drv_dma.o(i.app_dma_irq_handler) refers to drv_dma.o(i.drv_dma_irq_handler) for drv_dma_irq_handler
    drv_dma.o(i.drv_dma_abort_transfer) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_abort_transfer) refers to drv_dma.o(i.drv_dma_disenable_channel_interrupts) for drv_dma_disenable_channel_interrupts
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_disenable_channel_interrupts) for drv_dma_disenable_channel_interrupts
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_clear_flag) for drv_dma_clear_flag
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_set_ccr) for drv_dma_set_ccr
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_dma.o(i.drv_dma_clear_flag) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.drv_dma_create_handle) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dma.o(i.drv_dma_disenable_channel_interrupts) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.drv_dma_enable_channel_interrupts) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dma.o(i.drv_dma_enable_cycle) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_get_remaining_bytes) refers to drv_dma.o(i.drv_dma_channel_is_active) for drv_dma_channel_is_active
    drv_dma.o(i.drv_dma_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dma.o(i.drv_dma_init) refers to drv_dma.o(i.drv_dma_ahb_init) for drv_dma_ahb_init
    drv_dma.o(i.drv_dma_irq_handler) refers to drv_dma.o(i.drv_dma_get_channel_flag) for drv_dma_get_channel_flag
    drv_dma.o(i.drv_dma_irq_handler) refers to drv_dma.o(i.drv_dma_clear_flag) for drv_dma_clear_flag
    drv_dma.o(i.drv_dma_irq_handler) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_m2m_init) refers to memseta.o(.text) for __aeabi_memclr4
    drv_dma.o(i.drv_dma_m2m_init) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    drv_dma.o(i.drv_dma_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_dma.o(i.drv_dma_set_burst) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_set_transfer) refers to drv_dma.o(i.drv_dma_set_burst) for drv_dma_set_burst
    drv_dma.o(i.drv_dma_start_transfer) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    drv_dma.o(i.drv_dma_start_transfer) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_fls.o(i.drv_fls_gpio_connect) refers to drv_fls.o(i.drv_fls_gpio_disconnect) for drv_fls_gpio_disconnect
    drv_fls.o(i.drv_fls_gpio_disconnect) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_EnableClk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_busy_pending) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    drv_fls.o(i.fls_de_init) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    drv_fls.o(i.fls_de_init) refers to drv_dma.o(i.drv_dma_clear_flag) for drv_dma_clear_flag
    drv_fls.o(i.fls_de_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_disable_it) refers to drv_fls.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_fls.o(i.fls_disable_it) refers to drv_fls.o(i.fls_set_mc_irq_mask) for fls_set_mc_irq_mask
    drv_fls.o(i.fls_enable_it) refers to drv_fls.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_fls.o(i.fls_enable_it) refers to drv_fls.o(i.fls_set_mc_irq_mask) for fls_set_mc_irq_mask
    drv_fls.o(i.fls_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_init) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_spi_init) for fls_spi_init
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_ctrl_cfg_init) for fls_ctrl_cfg_init
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_set_tuning) for fls_set_tuning
    drv_fls.o(i.fls_init) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_enable_it) for fls_enable_it
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_set_mc_irq_mask) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_fls.o(i.fls_set_mc_irq_mask) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_set_write) for fls_set_write
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_set_write) for fls_set_write
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect) for drv_ap_rst_trig_edge_detect
    drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_get_pull_state) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_register_ap_reset_callback) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.drv_gpio_register_callback) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_set_driving_strength) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_gpio.o(i.drv_gpio_set_pull_state) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_set_schmitt_trigger) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_set_slew_rate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_i2c_dma.o(i.drv_i2c_dma_callback) refers to drv_i2c_dma.o(.data) for .data
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_i2c_master.o(i.drv_i2c_m_enable) for drv_i2c_m_enable
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req) for drv_sys_cfg_set_dma_rx_req
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_dma.o(i.drv_dma_set_transfer) for drv_dma_set_transfer
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_i2c_dma.o(i.drv_i2c_master_write_read_cmd) for drv_i2c_master_write_read_cmd
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_dma.o(i.drv_dma_set_transfer) for drv_dma_set_transfer
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_i2c_dma.o(.data) for .data
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_i2c_dma.o(.bss) for .bss
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_i2c_dma.o(i.drv_i2c_dma_callback) for drv_i2c_dma_callback
    drv_i2c_dma.o(i.drv_i2c_slave_write_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_i2c_master.o(i.app_I2C1_IRQn_Handler) refers to drv_i2c_master.o(.data) for .data
    drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_enable_intr) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_read_data) refers to drv_i2c_master.o(i.drv_i2c_m_get_fifo_status) for drv_i2c_m_get_fifo_status
    drv_i2c_master.o(i.drv_i2c_m_set_callback) refers to drv_i2c_master.o(.data) for .data
    drv_i2c_master.o(i.drv_i2c_m_set_sys_mask) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_write_data) refers to drv_i2c_master.o(i.drv_i2c_m_get_fifo_status) for drv_i2c_m_get_fifo_status
    drv_i2c_master.o(i.drv_i2c_master_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_i2c_master.o(i.drv_i2c_master_init) refers to drv_common.o(.data) for g_system_clock
    drv_i2c_slave.o(i.app_I2C0_IRQn_Handler) refers to drv_i2c_slave.o(.data) for .data
    drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit) refers to drv_i2c_slave.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_slave.o(i.drv_i2c_s_enable_intr) refers to drv_i2c_slave.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_slave.o(i.drv_i2c_s_get_tx_byte_num) refers to drv_i2c_slave.o(.data) for .data
    drv_i2c_slave.o(i.drv_i2c_s_read_data) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    drv_i2c_slave.o(i.drv_i2c_s_set_callback) refers to drv_i2c_slave.o(.data) for .data
    drv_i2c_slave.o(i.drv_i2c_s_set_sys_mask) refers to drv_i2c_slave.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_slave.o(i.drv_i2c_s_write_data) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    drv_param_init.o(i.drv_param_init_get_ccm) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_get_scld_filter_h) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_get_scld_filter_v) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_get_sclu_filter) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_set_ccm) refers to memcpya.o(.text) for __aeabi_memcpy4
    drv_param_init.o(i.drv_param_init_set_ccm) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_set_scld_filter) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_set_sclu_filter) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_p2r_filter_init) refers to drv_param_init.o(.constdata) for .constdata
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_dma.o(i.drv_dma_disenable_channel_interrupts) for drv_dma_disenable_channel_interrupts
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_master.o(i.drv_spi_m_enable_rx_dma) for drv_spi_m_enable_rx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_slave.o(i.drv_spi_s_enable_tx_dma) for drv_spi_s_enable_tx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_slave.o(i.drv_spi_s_enable_rx_dma) for drv_spi_s_enable_rx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_dma.o(i.drv_spi_dma_callback) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_dma_ch6_init) refers to drv_spi_dma.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_dma.o(i.drv_spi_dma_ch6_init) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_dma_init) refers to drv_spi_dma.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_dma.o(i.drv_spi_dma_init) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_spi_dma.o(i.drv_spi_dma_callback) for drv_spi_dma_callback
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_spi_dma.o(i.drv_spi_dma_callback) for drv_spi_dma_callback
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_spi_master.o(i.drv_spi_m_enable_rx_dma) for drv_spi_m_enable_rx_dma
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_spi_slave.o(i.drv_spi_s_enable_tx_dma) for drv_spi_s_enable_tx_dma
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_master.o(i.app_SPIM_IRQn_Handler) refers to drv_spi_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_master.o(i.app_SPIM_IRQn_Handler) refers to drv_spi_master.o(.data) for .data
    drv_spi_master.o(i.drv_spi_m_deinit) refers to drv_spi_master.o(i.drv_spi_m_switch_sclk) for drv_spi_m_switch_sclk
    drv_spi_master.o(i.drv_spi_m_disable_int) refers to drv_spi_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_master.o(i.drv_spi_m_set_intr_callback) refers to drv_spi_master.o(.data) for .data
    drv_spi_master.o(i.drv_spi_master_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_spi_master.o(i.drv_spi_master_init) refers to drv_common.o(.data) for g_system_clock
    drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig) for drv_sys_cfg_sel_ap_rst_lvl_trig
    drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect) refers to drv_sys_cfg.o(.data) for .data
    drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig) for drv_sys_cfg_sel_ap_rst_lvl_trig
    drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) refers to drv_sys_cfg.o(.data) for .data
    drv_timer.o(i.app_TIMER0_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.app_TIMER1_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.app_TIMER2_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.app_TIMER3_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.drv_timer_clean_timer_value) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_timer.o(i.drv_timer_enable) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_get_current_count) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_get_instance) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_get_match) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_get_prescaler) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_clear_status_flags) for drv_timer_clear_status_flags
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_match) for drv_timer_set_match
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_current_count) for drv_timer_set_current_count
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_register_callback) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_current_count) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_timer.o(i.drv_timer_set_match) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_repeat) refers to drv_timer.o(.data) for .data
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to hal_internal_vsync.o(i.soft_gen_te) for soft_gen_te
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_param_init.o(i.drv_param_init_get_ccm) for drv_param_init_get_ccm
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_lcdc.o(i.drv_lcdc_config_ccm) for drv_lcdc_config_ccm
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to ddiv.o(.text) for __aeabi_ddiv
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to sqrt.o(i.sqrt) for sqrt
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to dmul.o(.text) for __aeabi_dmul
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to cdcmple.o(.text) for __aeabi_cdcmple
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to hal_internal_vsync.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.dcs_sw_filter) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_iniernal_vsync_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.hal_iniernal_vsync_deinit) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_mode) for drv_memc_set_ltpo_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_double_buffer) for drv_memc_set_double_buffer
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_active_height) for drv_memc_set_active_height
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_inten) for drv_memc_set_inten
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) for hal_dsi_rx_ctrl_gen_a_tear_signal
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_delay.o(i.delayUs) for delayUs
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.hal_internal_init_memc) for hal_internal_init_memc
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_chip_info.o(i.drv_chip_rx_info_check) for drv_chip_rx_info_check
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_rxbr.o(i.drv_rxbr_register_irq0_callback) for drv_rxbr_register_irq0_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_rxbr.o(i.drv_rxbr_register_irq1_callback) for drv_rxbr_register_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_vidc.o(i.drv_vidc_register_callback) for drv_vidc_register_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_init) for dcs_packet_fifo_init
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.rxbr_irq0_callback) for rxbr_irq0_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.rxbr_irq1_callback) for rxbr_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.vidc_callback) for vidc_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) refers to drv_rxbr.o(i.drv_rxbr_set_cmd_filter) for drv_rxbr_set_cmd_filter
    hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) for hal_internal_vsync_set_auto_hw_filter
    hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(i.vsync_set_te_mode) for vsync_set_te_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.vsync_set_te_mode) for vsync_set_te_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(i.dcs_sw_filter) for dcs_sw_filter
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) for dcs_packet_fifo_alloc
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) for hal_dsi_rx_ctrl_dsc_async_handler
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_rxbr.o(i.drv_rxbr_get_col_addr) for drv_rxbr_get_col_addr
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_rxbr.o(i.drv_rxbr_get_page_addr) for drv_rxbr_get_page_addr
    hal_internal_vsync.o(i.rx_partial_update) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_dsc_dec.o(i.drv_dsc_dec_get_nslc) for drv_dsc_dec_get_nslc
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_crgu.o(i.drv_crgu_set_dsco_src) for drv_crgu_set_dsco_src
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_crgu.o(i.drv_crgu_set_dsco_src_div) for drv_crgu_set_dsco_src_div
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_crgu.o(i.drv_crgu_set_dsc_core_div) for drv_crgu_set_dsc_core_div
    hal_internal_vsync.o(i.rx_partial_update) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(i.rx_get_dcs_packet_data) for rx_get_dcs_packet_data
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(i.rx_receive_pps) for rx_receive_pps
    hal_internal_vsync.o(i.rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_receive_pps) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.rx_receive_pps) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rx_receive_pps) refers to hal_internal_vsync.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter) for drv_dsc_dec_convert_pps_rc_parameter
    hal_internal_vsync.o(i.rx_receive_pps) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps) for drv_dsc_dec_set_u8_pps
    hal_internal_vsync.o(i.rx_receive_pps) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.rx_receive_pps) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.rx_receive_packet) for rx_receive_packet
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_int_source) for drv_rxbr_get_int_source
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.rx_partial_update) for rx_partial_update
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_int_source) for drv_rxbr_get_int_source
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.vpre_err_reset) for vpre_err_reset
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_memc.o(i.drv_memc_set_double_buffer_reverse) for drv_memc_set_double_buffer_reverse
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_get_irq_status) for drv_vidc_get_irq_status
    hal_internal_vsync.o(i.vidc_callback) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_clear_irq) for drv_vidc_clear_irq
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_internal_vsync.o(i.vidc_callback) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps) for drv_dsc_dec_set_u8_pps
    hal_internal_vsync.o(i.vpre_err_reset) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to drv_lcdc.o(i.drv_lcdc_ctrl_flow) for drv_lcdc_ctrl_flow
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(.data) refers to hal_internal_vsync.o(.bss) for sg_te_info
    dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_fifo_init) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_size) refers to dcs_packet_fifo.o(.bss) for .bss
    drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to ffltui.o(.text) for __aeabi_ui2f
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fdiv.o(.text) for __aeabi_fdiv
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fmul.o(.text) for __aeabi_fmul
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) for drv_dsi_rx_get_color_bpp
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc) for drv_dsi_rx_get_color_pcc
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fadd.o(.text) for __aeabi_fadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to cfrcmple.o(.text) for __aeabi_cfrcmple
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to f2d.o(.text) for __aeabi_f2d
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dadd.o(.text) for __aeabi_dadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dfixui.o(.text) for __aeabi_d2uiz
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte) for drv_rx_phy_test_write_1_byte
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to drv_dsi_rx.o(i.drv_rx_phy_test_read) for drv_rx_phy_test_read
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap) refers to drv_chip_info.o(i.drv_chip_info_get_info) for drv_chip_info_get_info
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_get_rate_para) for drv_phy_get_rate_para
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_get_calibration) for drv_phy_get_calibration
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_clear) for drv_rx_phy_test_clear
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte) for drv_rx_phy_test_write_1_byte
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte) for drv_rx_phy_test_write_2_byte
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_chip_info.o(i.drv_chip_info_get_info) for drv_chip_info_get_info
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_lock) for drv_rx_phy_test_lock
    drv_dsi_rx.o(i.drv_rx_phy_test_clear) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_rx.o(i.drv_rx_phy_test_lock) refers to drv_phy_common.o(i.drv_phy_test_lock) for drv_phy_test_lock
    drv_dsi_rx.o(i.drv_rx_phy_test_read) refers to drv_phy_common.o(i.drv_phy_test_read) for drv_phy_test_read
    drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_1_byte) for drv_phy_test_write_1_byte
    drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_2_byte) for drv_phy_test_write_2_byte
    drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) for drv_tx_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to drv_dsi_tx.o(i.drv_tx_phy_test_read) for drv_tx_phy_test_read
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_get_rate_para) for drv_phy_get_rate_para
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_get_pll_para) for drv_phy_get_pll_para
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_get_calibration) for drv_phy_get_calibration
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_enter) for drv_tx_phy_test_enter
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_crgu.o(i.drv_crgu_set_mipi_ref_src) for drv_crgu_set_mipi_ref_src
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_crgu.o(i.drv_crgu_set_mipi_cfg_src) for drv_crgu_set_mipi_cfg_src
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_clear) for drv_tx_phy_test_clear
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) for drv_tx_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte) for drv_tx_phy_test_write_2_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_code) for drv_tx_phy_test_write_code
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_exit) for drv_tx_phy_test_exit
    drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) for drv_tx_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_version) for drv_dsi_tx_version
    drv_dsi_tx.o(i.drv_dsi_tx_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dsi_tx.o(i.drv_tx_phy_test_clear) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_tx.o(i.drv_tx_phy_test_read) refers to drv_phy_common.o(i.drv_phy_test_read) for drv_phy_test_read
    drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_1_byte) for drv_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_2_byte) for drv_phy_test_write_2_byte
    drv_dsi_tx.o(i.drv_tx_phy_test_write_code) refers to drv_phy_common.o(i.drv_phy_test_write_code) for drv_phy_test_write_code
    drv_lcdc.o(i.drv_lcdc_config_src_parameter) refers to drv_lcdc.o(i.drv_lcdc_config_input_size) for drv_lcdc_config_input_size
    drv_lcdc.o(i.drv_lcdc_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_memc.o(i.app_MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_get_status) for drv_memc_get_status
    drv_memc.o(i.app_MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_clear_status) for drv_memc_clear_status
    drv_memc.o(i.app_MEMC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_rxbr.o(i.app_ADC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.app_ADC_IRQn_Handler) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.app_VPRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.app_VPRE_IRQn_Handler) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_EnableIRQ) for __NVIC_EnableIRQ
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_rxbr.o(i.drv_rxbr_register_irq0_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_register_irq1_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_set_cmd_filter) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_rxbr.o(i.drv_rxbr_soft_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_vidc.o(i.app_VIDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.app_VIDC_IRQn_Handler) refers to drv_vidc.o(.data) for .data
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_vidc.o(i.drv_vidc_register_callback) refers to drv_vidc.o(.data) for .data
    irq_redirect .o(i.ADC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.AP_NRESET_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.DMA_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT0_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT1_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT2_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT3_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT4_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT5_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT6_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT7_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.FLSCTRL_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.HardFault_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.I2C0_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.I2C1_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.LCDC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.MEMC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.MIPI_RX_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.MIPI_TX_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.PWMDET_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SPIM_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SPIS_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SWIRE_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SysTick_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER0_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER1_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER2_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER3_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.UART_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.VIDC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.VPRE_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.WDG_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.handle_init) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.handle_init) refers to drv_common.o(i.app_SysTick_Handler) for app_SysTick_Handler
    irq_redirect .o(i.handle_init) refers to hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) for app_LCDC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler) for app_MIPI_RX_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler) for app_MIPI_TX_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_dma.o(i.app_dma_irq_handler) for app_dma_irq_handler
    irq_redirect .o(i.handle_init) refers to norflash.o(i.app_fls_ctrl_Handler) for app_fls_ctrl_Handler
    irq_redirect .o(i.handle_init) refers to drv_i2c_slave.o(i.app_I2C0_IRQn_Handler) for app_I2C0_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_i2c_master.o(i.app_I2C1_IRQn_Handler) for app_I2C1_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to hal_spi_slave.o(i.app_SPIS_IRQn_Handler) for app_SPIS_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_spi_master.o(i.app_SPIM_IRQn_Handler) for app_SPIM_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_rxbr.o(i.app_VPRE_IRQn_Handler) for app_VPRE_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_rxbr.o(i.app_ADC_IRQn_Handler) for app_ADC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_vidc.o(i.app_VIDC_IRQn_Handler) for app_VIDC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_memc.o(i.app_MEMC_IRQn_Handler) for app_MEMC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER0_IRQn_Handler) for app_TIMER0_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER1_IRQn_Handler) for app_TIMER1_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER2_IRQn_Handler) for app_TIMER2_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER3_IRQn_Handler) for app_TIMER3_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_wdg.o(i.app_WDG_IRQn_Handler) for app_WDG_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_uart.o(i.app_UART_IRQn_Handler) for app_UART_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_pwm.o(i.app_PWMDET_IRQn_Handler) for app_PWMDET_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_swire.o(i.app_SWIRE_IRQn_Handler) for app_SWIRE_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) for app_AP_NRESET_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler) for app_EXTI_INT0_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler) for app_EXTI_INT1_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler) for app_EXTI_INT2_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler) for app_EXTI_INT3_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler) for app_EXTI_INT4_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler) for app_EXTI_INT5_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler) for app_EXTI_INT6_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler) for app_EXTI_INT7_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_common.o(i.app_HardFault_Handler) for app_HardFault_Handler
    drv_phy_common.o(i.drv_phy_enable_calibration) refers to drv_phy_common.o(.data) for .data
    drv_phy_common.o(i.drv_phy_get_calibration) refers to drv_chip_info.o(i.drv_chip_info_get_info) for drv_chip_info_get_info
    drv_phy_common.o(i.drv_phy_get_calibration) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_phy_common.o(i.drv_phy_get_calibration) refers to drv_phy_common.o(.data) for .data
    drv_phy_common.o(i.drv_phy_get_pll_para) refers to drv_phy_common.o(.constdata) for .constdata
    drv_phy_common.o(i.drv_phy_get_rate_para) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_phy_common.o(i.drv_phy_get_rate_para) refers to drv_phy_common.o(.constdata) for .constdata
    drv_phy_common.o(i.drv_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_code) for drv_phy_test_write_code
    drv_phy_common.o(i.drv_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_data) for drv_phy_test_write_data
    drv_phy_common.o(i.drv_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_code) for drv_phy_test_write_code
    drv_phy_common.o(i.drv_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_data) for drv_phy_test_write_data
    drv_chip_info.o(i.drv_chip_info_get_info) refers to drv_chip_info.o(.data) for .data
    drv_chip_info.o(i.drv_chip_info_init) refers to drv_efuse.o(i.drv_efuse_enter_inactive) for drv_efuse_enter_inactive
    drv_chip_info.o(i.drv_chip_info_init) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_chip_info.o(i.drv_chip_info_init) refers to drv_chip_info.o(.data) for .data
    drv_chip_info.o(i.drv_chip_rx_info_check) refers to printfa.o(i.__0printf) for __2printf
    drv_chip_info.o(i.drv_chip_rx_info_check) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_chip_info.o(i.drv_chip_rx_info_check) refers to drv_chip_info.o(.data) for .data
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to drv_efuse.o(i.drv_efuse_enter_inactive) for drv_efuse_enter_inactive
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to printfa.o(i.__0printf) for __2printf
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to hal_spi_slave.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_spi_slave.o(i.hal_spi_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    hal_spi_slave.o(i.hal_spi_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_abort) refers to drv_spi_dma.o(i.drv_spi_abort_dma) for drv_spi_abort_dma
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start) refers to drv_dma.o(i.drv_dma_enable_cycle) for drv_dma_enable_cycle
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start) refers to drv_spi_dma.o(i.drv_spis_dma_write) for drv_spis_dma_write
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_deinit) refers to drv_spi_slave.o(i.drv_spi_s_deinit) for drv_spi_s_deinit
    hal_spi_slave.o(i.hal_spi_slave_enable) refers to drv_spi_slave.o(i.drv_spi_s_enable_int) for drv_spi_s_enable_int
    hal_spi_slave.o(i.hal_spi_slave_enable) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_spi_slave.o(i.hal_spi_slave_enable) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_gpio_init) refers to drv_spi_slave.o(i.drv_spi_s_gpio_init) for drv_spi_s_gpio_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to hal_spi_slave.o(i.hal_spi_slave_gpio_init) for hal_spi_slave_gpio_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_slave.o(i.drv_spi_slave_init) for drv_spi_slave_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_dma.o(i.drv_spi_dma_init) for drv_spi_dma_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) for drv_spi_set_dma_irq_callback
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_slave.o(i.drv_spi_s_enable_tx_dma) for drv_spi_s_enable_tx_dma
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    hal_spi_slave.o(i.hal_spi_slave_init) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_read_data) refers to drv_spi_slave.o(i.drv_spi_s_read_data) for drv_spi_s_read_data
    hal_spi_slave.o(i.hal_spi_slave_register_callback) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_reset_tx) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_set_auto_rx_buffer) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_set_auto_tx_buffer) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_write_data) refers to drv_spi_slave.o(i.drv_spi_s_write_data) for drv_spi_s_write_data
    drv_fls_dma.o(i.fls_abort_dma) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_fls_dma.o(i.fls_abort_dma) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls_dma.o(i.fls_dma_enable) for fls_dma_enable
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_set_write) for fls_set_write
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls_dma.o(i.fls_dma_enable) for fls_dma_enable
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls_dma.o(i.fls_read_dmacallback) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to memseta.o(.text) for __aeabi_memclr4
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_fls_dma.o(.data) for .data
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_fls_dma.o(i.fls_read_dmacallback) for fls_read_dmacallback
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_fls_dma.o(i.fls_write_dmacallback) for fls_write_dmacallback
    drv_fls_dma.o(i.fls_transfer_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_fls_dma.o(i.fls_transfer_dma) refers to drv_dma.o(i.drv_dma_start_transfer) for drv_dma_start_transfer
    drv_fls_dma.o(i.fls_transfer_get_receive_count_dma) refers to drv_dma.o(i.drv_dma_get_remaining_bytes) for drv_dma_get_remaining_bytes
    drv_fls_dma.o(i.fls_write_dmacallback) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_pwm.o(i.app_PWMDET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_pwm.o(i.app_PWMDET_IRQn_Handler) refers to drv_pwm.o(.data) for .data
    drv_pwm.o(i.drv_pwm_in_register_callback) refers to drv_pwm.o(.data) for .data
    drv_pwm.o(i.drv_pwm_in_set_sys_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_spi_slave.o(i.drv_spi_s_deinit) refers to drv_spi_slave.o(i.drv_spi_s_switch_sclk) for drv_spi_s_switch_sclk
    drv_swire.o(i.app_SWIRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_swire.o(i.app_SWIRE_IRQn_Handler) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    drv_swire.o(i.app_SWIRE_IRQn_Handler) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_register_callback) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.UART0_IRQ_Handle) refers to drv_uart.o(i.UART_TransferHandleIRQ) for UART_TransferHandleIRQ
    drv_uart.o(i.UART0_IRQ_Handle) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_uart.o(i.UART0_IRQ_Handle) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_AbortReceive) refers to drv_uart.o(i.UART_Disable_IT) for UART_Disable_IT
    drv_uart.o(i.UART_AbortReceive) refers to drv_uart.o(i.UART_ResetRxFIFO) for UART_ResetRxFIFO
    drv_uart.o(i.UART_AbortSend) refers to drv_uart.o(i.UART_Disable_IT) for UART_Disable_IT
    drv_uart.o(i.UART_AbortSend) refers to drv_uart.o(i.UART_ResetTxFIFO) for UART_ResetTxFIFO
    drv_uart.o(i.UART_Deinit) refers to drv_uart.o(i.UART_SwitchSCLK) for UART_SwitchSCLK
    drv_uart.o(i.UART_Disable_IT) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_Disable_IT) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.UART_Disable_IT) refers to drv_uart.o(.constdata) for .constdata
    drv_uart.o(i.UART_EnableDma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req) for drv_sys_cfg_set_dma_rx_req
    drv_uart.o(i.UART_EnableDma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    drv_uart.o(i.UART_Enable_IT) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_Enable_IT) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.UART_GetDefaultConfig) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.UART_GetDefaultConfig) refers to drv_common.o(.data) for g_system_clock
    drv_uart.o(i.UART_GetFIFO_Ctrl) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_GetFIFO_Ctrl) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_ResetRxFIFO) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_ResetRxFIFO) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_ResetTxFIFO) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_ResetTxFIFO) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_SetBaudRate) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_uart.o(i.UART_SwitchSCLK) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_uart.o(i.UART_TransferCreateHandle) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_TransferCreateHandle) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.UART_TransferCreateHandle) refers to drv_uart.o(i.UART_Enable_IT) for UART_Enable_IT
    drv_uart.o(i.UART_TransferCreateHandle) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_TransferHandleIRQ) refers to drv_uart.o(i.UART_ResetRxFIFO) for UART_ResetRxFIFO
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_DisableDma) for UART_DisableDma
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_SwitchSCLK) for UART_SwitchSCLK
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_SetBaudRate) for UART_SetBaudRate
    drv_uart.o(i.UART_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.UART_init) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.app_UART_IRQn_Handler) refers to drv_uart.o(i.UART0_IRQ_Handle) for UART0_IRQ_Handle
    drv_uart_dma.o(i.UART_DMAInit) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart_dma.o(i.UART_DMAInit) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    drv_uart_dma.o(i.UART_TransferAbortReceiveDMA) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_uart_dma.o(i.UART_TransferAbortSendDMA) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart.o(i.UART_EnableDma) for UART_EnableDma
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(i.UART_DMAInit) for UART_DMAInit
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(.data) for .data
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(i.UART_TransferReceiveDMACallback) for UART_TransferReceiveDMACallback
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(i.UART_TransferSendDMACallback) for UART_TransferSendDMACallback
    drv_uart_dma.o(i.UART_TransferGetReceiveCountDMA) refers to drv_dma.o(i.drv_dma_get_remaining_bytes) for drv_dma_get_remaining_bytes
    drv_uart_dma.o(i.UART_TransferReceiveDMA) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_uart_dma.o(i.UART_TransferReceiveDMA) refers to drv_uart.o(i.UART_EnableDma) for UART_EnableDma
    drv_uart_dma.o(i.UART_TransferReceiveDMA) refers to drv_dma.o(i.drv_dma_start_transfer) for drv_dma_start_transfer
    drv_uart_dma.o(i.UART_TransferSendDMA) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_uart_dma.o(i.UART_TransferSendDMA) refers to drv_uart.o(i.UART_EnableDma) for UART_EnableDma
    drv_uart_dma.o(i.UART_TransferSendDMA) refers to drv_dma.o(i.drv_dma_start_transfer) for drv_dma_start_transfer
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_set_int) for drv_wdg_set_int
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_clear_counter) for drv_wdg_clear_counter
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_read_edge_flag) for drv_wdg_read_edge_flag
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_clear_edge_flag) for drv_wdg_clear_edge_flag
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(.data) for .data
    drv_wdg.o(i.drv_wdg_register_callback) refers to drv_wdg.o(.data) for .data
    drv_wdg.o(i.drv_wdg_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_wdg.o(i.drv_wdg_set_repeat) refers to drv_wdg.o(.data) for .data
    drv_efuse.o(i.drv_efuse_enter_inactive) refers to drv_efuse.o(i.drv_efuse_int_enable) for drv_efuse_int_enable
    drv_efuse.o(i.drv_efuse_read) refers to drv_efuse.o(i.drv_efuse_read_req) for drv_efuse_read_req
    drv_efuse.o(i.drv_efuse_write) refers to drv_efuse.o(i.drv_efuse_write_req) for drv_efuse_write_req
    ceil.o(i.__softfp_ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.__softfp_ceil) refers to ceil.o(i.ceil) for ceil
    ceil.o(i.ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.ceil) refers to dadd.o(.text) for __aeabi_dadd
    ceil.o(i.ceil) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    sqrt.o(i.__softfp_sqrt) refers (Special) to iusefp.o(.text) for __I$use$fp
    sqrt.o(i.__softfp_sqrt) refers to dsqrt.o(.text) for _dsqrt
    sqrt.o(i.__softfp_sqrt) refers to errno.o(i.__set_errno) for __set_errno
    sqrt.o(i.sqrt) refers (Special) to iusefp.o(.text) for __I$use$fp
    sqrt.o(i.sqrt) refers to dsqrt.o(.text) for _dsqrt
    sqrt.o(i.sqrt) refers to errno.o(i.__set_errno) for __set_errno
    sqrt_x.o(i.____softfp_sqrt$lsc) refers (Special) to iusefp.o(.text) for __I$use$fp
    sqrt_x.o(i.____softfp_sqrt$lsc) refers to cdcmple.o(.text) for __aeabi_cdcmple
    sqrt_x.o(i.____softfp_sqrt$lsc) refers to errno.o(i.__set_errno) for __set_errno
    sqrt_x.o(i.____softfp_sqrt$lsc) refers to dsqrt.o(.text) for _dsqrt
    sqrt_x.o(i.__sqrt$lsc) refers (Special) to iusefp.o(.text) for __I$use$fp
    sqrt_x.o(i.__sqrt$lsc) refers to cdcmple.o(.text) for __aeabi_cdcmple
    sqrt_x.o(i.__sqrt$lsc) refers to errno.o(i.__set_errno) for __set_errno
    sqrt_x.o(i.__sqrt$lsc) refers to dsqrt.o(.text) for _dsqrt
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry10a.o(.ARM.Collect$$$$0000000D) for __rt_final_cpp
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry11a.o(.ARM.Collect$$$$0000000F) for __rt_final_exit
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry7b.o(.ARM.Collect$$$$00000008) for _main_clock
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry8b.o(.ARM.Collect$$$$0000000A) for _main_cpp_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry9a.o(.ARM.Collect$$$$0000000B) for _main_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry5.o(.ARM.Collect$$$$00000004) for _main_scatterload
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry2.o(.ARM.Collect$$$$00000001) for _main_stk
    idiv.o(.text) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfb.o(i.__0fprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0fprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0printf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printfb.o(i.__0vfprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vfprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printf0.o(i.__0fprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0fprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0printf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf0.o(i.__0vfprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vfprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf1.o(i.__0fprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0fprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0printf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i.__0vfprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vfprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf2.o(i.__0fprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0fprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0printf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf2.o(i.__0vfprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vfprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf3.o(i.__0fprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0fprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0printf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i.__0vfprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vfprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf4.o(i.__0fprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0fprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0printf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i.__0vfprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vfprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf5.o(i.__0fprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0fprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0printf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i.__0vfprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vfprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf6.o(i.__0fprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0fprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0printf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i.__0vfprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vfprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i._printf_core) refers to printf6.o(i._printf_pre_padding) for _printf_pre_padding
    printf6.o(i._printf_core) refers to printf6.o(i._printf_post_padding) for _printf_post_padding
    printf6.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf7.o(i.__0fprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0fprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0printf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i.__0vfprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vfprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i._printf_core) refers to printf7.o(i._printf_pre_padding) for _printf_pre_padding
    printf7.o(i._printf_core) refers to printf7.o(i._printf_post_padding) for _printf_post_padding
    printf7.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf8.o(i.__0fprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0fprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0printf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i.__0vfprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vfprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i._printf_core) refers to printf8.o(i._printf_pre_padding) for _printf_pre_padding
    printf8.o(i._printf_core) refers to printf8.o(i._printf_post_padding) for _printf_post_padding
    printf8.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i.__0fprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0fprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0fprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0printf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0printf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0snprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0snprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0snprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0sprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0sprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0sprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i.__0vfprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vfprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vfprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0vsnprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0vsprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i._fp_digits) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._fp_digits) refers to dmul.o(.text) for __aeabi_dmul
    printfa.o(i._fp_digits) refers to ddiv.o(.text) for __aeabi_ddiv
    printfa.o(i._fp_digits) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    printfa.o(i._fp_digits) refers to dadd.o(.text) for __aeabi_dadd
    printfa.o(i._fp_digits) refers to dfixul.o(.text) for __aeabi_d2ulz
    printfa.o(i._fp_digits) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_core) refers to printfa.o(i._printf_pre_padding) for _printf_pre_padding
    printfa.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers to printfa.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i._printf_core) refers to printfa.o(i._fp_digits) for _fp_digits
    printfa.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfa.o(i._printf_post_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_pre_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._snputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._sputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    fmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers to fepilogue.o(.text) for _float_round
    fscalb.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    dadd.o(.text) refers to llsshr.o(.text) for __aeabi_lasr
    dadd.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dmul.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ddiv.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ddiv.o(.text) refers to depilogue.o(.text) for _double_round
    fflti.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fflti.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    ffltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ffltui.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    dflti.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dflti.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dfltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfltui.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ffixi.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ffixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixi.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixi.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixui.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    f2d.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    cdcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    cfrcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    entry2.o(.ARM.Collect$$$$00000001) refers to entry2.o(.ARM.Collect$$$$00002712) for __lit__00000000
    entry2.o(.ARM.Collect$$$$00002712) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    entry5.o(.ARM.Collect$$$$00000004) refers to init.o(.text) for __scatterload
    entry9a.o(.ARM.Collect$$$$0000000B) refers to main.o(i.main) for main
    entry9b.o(.ARM.Collect$$$$0000000C) refers to main.o(i.main) for main
    uldiv.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    uldiv.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    errno.o(i.__aeabi_errno_addr) refers to errno.o(.data) for .data
    errno.o(i.__read_errno) refers to errno.o(.data) for .data
    errno.o(i.__set_errno) refers to errno.o(.data) for .data
    depilogue.o(.text) refers to depilogue.o(i.__ARM_clz) for __ARM_clz
    depilogue.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dsqrt.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dsqrt.o(.text) refers to depilogue.o(.text) for _double_round
    dfixul.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixul.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    init.o(.text) refers to entry5.o(.ARM.Collect$$$$00000004) for __main_after_scatterload


==============================================================================

Removing Unused input sections from the image.

    Removing main.o(.rev16_text), (4 bytes).
    Removing main.o(.revsh_text), (4 bytes).
    Removing ap_demo.o(.rev16_text), (4 bytes).
    Removing ap_demo.o(.revsh_text), (4 bytes).
    Removing ap_demo.o(.data), (256 bytes).
    Removing ap_demo.o(.data), (256 bytes).
    Removing ap_demo.o(.data), (2 bytes).
    Removing ap_demo.o(.data), (2 bytes).
    Removing ap_demo.o(.data), (2 bytes).
    Removing ap_demo.o(.data), (2 bytes).
    Removing app_tp_transfer.o(.rev16_text), (4 bytes).
    Removing app_tp_transfer.o(.revsh_text), (4 bytes).
    Removing app_tp_transfer.o(i.app_tp_m_transfer_complate), (8 bytes).
    Removing app_tp_transfer.o(i.app_tp_phone_reset_on), (12 bytes).
    Removing app_tp_transfer.o(i.app_tp_s_transfer_complate), (26 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (5 bytes).
    Removing app_tp_transfer.o(.data), (6 bytes).
    Removing app_tp_transfer.o(.data), (2 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (4 bytes).
    Removing app_tp_transfer.o(.data), (4 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (1 bytes).
    Removing app_tp_transfer.o(.data), (2 bytes).
    Removing app_tp_transfer.o(.data), (2 bytes).
    Removing app_tp_st_touch.o(.rev16_text), (4 bytes).
    Removing app_tp_st_touch.o(.revsh_text), (4 bytes).
    Removing app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset), (196 bytes).
    Removing board.o(.rev16_text), (4 bytes).
    Removing board.o(.revsh_text), (4 bytes).
    Removing startup_armcm0.o(HEAP), (3072 bytes).
    Removing hal_dsi_rx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd), (88 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_short_cmd), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video), (228 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init), (48 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern), (216 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en), (16 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode), (128 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle), (40 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart), (80 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_dcs_direct_mode), (8 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter), (40 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode), (52 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format), (56 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data), (148 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk), (68 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_te_waveform), (52 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate), (112 bytes).
    Removing hal_dsi_tx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic), (144 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_ulps_mode), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_ulps_mode), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd), (140 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle), (28 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_pq_filter), (24 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_lp_cmd), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg), (24 bytes).
    Removing hal_gpio.o(.rev16_text), (4 bytes).
    Removing hal_gpio.o(.revsh_text), (4 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_int_type), (20 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_pull_state), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_driving_strength), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_output_data_ex), (36 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_schmitt_trigger), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_slew_rate), (32 bytes).
    Removing hal_i2c_master.o(.rev16_text), (4 bytes).
    Removing hal_i2c_master.o(.revsh_text), (4 bytes).
    Removing hal_i2c_master.o(i.hal_i2c_m_set_high_impedance), (46 bytes).
    Removing hal_i2c_slave.o(.rev16_text), (4 bytes).
    Removing hal_i2c_slave.o(.revsh_text), (4 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_get_tx_byte_num), (8 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_read_complate), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_read_complate_clear), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_read_data), (8 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_rxfifo_notempty), (20 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_set_dma_tx_cycle), (36 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance), (46 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_write_complate), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_write_data), (8 bytes).
    Removing hal_spi_master.o(.rev16_text), (4 bytes).
    Removing hal_spi_master.o(.revsh_text), (4 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_callback), (24 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_dma_init), (104 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_dma_read), (36 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_dma_write), (40 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_get_transfer_complate), (36 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_gpio_init), (8 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_read_rxfifo), (28 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_set_high_impedance), (100 bytes).
    Removing hal_spi_master.o(.data), (1 bytes).
    Removing hal_system.o(.rev16_text), (4 bytes).
    Removing hal_system.o(.revsh_text), (4 bytes).
    Removing hal_system.o(i.hal_system_deep_sleep_mode), (8 bytes).
    Removing hal_system.o(i.hal_system_disable_systick), (8 bytes).
    Removing hal_system.o(i.hal_system_flash_read), (56 bytes).
    Removing hal_system.o(i.hal_system_flash_write), (58 bytes).
    Removing hal_system.o(i.hal_system_get_tick), (8 bytes).
    Removing hal_system.o(i.hal_system_idle_mode), (8 bytes).
    Removing hal_system.o(i.hal_system_register_systick_cb), (8 bytes).
    Removing hal_system.o(i.hal_system_reset_chip), (32 bytes).
    Removing hal_system.o(i.hal_system_share_flash_mode), (20 bytes).
    Removing hal_system.o(i.hal_system_sleep_mode), (48 bytes).
    Removing hal_timer.o(.rev16_text), (4 bytes).
    Removing hal_timer.o(.revsh_text), (4 bytes).
    Removing hal_timer.o(i.hal_timer_deinit), (46 bytes).
    Removing hal_timer.o(i.hal_timer_get_status), (52 bytes).
    Removing hal_timer.o(i.hal_timer_set_repeat), (8 bytes).
    Removing hal_timer.o(i.hal_timer_stop), (48 bytes).
    Removing tau_delay.o(.rev16_text), (4 bytes).
    Removing tau_delay.o(.revsh_text), (4 bytes).
    Removing tau_log.o(.rev16_text), (4 bytes).
    Removing tau_log.o(.revsh_text), (4 bytes).
    Removing tau_log.o(i.fgetc), (22 bytes).
    Removing app_tp_for_custom_s8.o(.rev16_text), (4 bytes).
    Removing app_tp_for_custom_s8.o(.revsh_text), (4 bytes).
    Removing app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const), (56 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (1120 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (1120 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (288 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (1 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (3 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (3 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (64 bytes).
    Removing app_tp_for_custom_s8.o(.data), (3 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (32 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing hal_uart.o(.rev16_text), (4 bytes).
    Removing hal_uart.o(.revsh_text), (4 bytes).
    Removing hal_uart.o(i.hal_uart_deinit), (28 bytes).
    Removing hal_uart.o(i.hal_uart_dmacallback), (36 bytes).
    Removing hal_uart.o(i.hal_uart_receive_blocking), (16 bytes).
    Removing hal_uart.o(i.hal_uart_receive_dma), (76 bytes).
    Removing hal_uart.o(i.hal_uart_transmit_dma), (76 bytes).
    Removing norflash.o(.rev16_text), (4 bytes).
    Removing norflash.o(.revsh_text), (4 bytes).
    Removing norflash.o(i.norflash_best_cfg_init), (44 bytes).
    Removing norflash.o(i.norflash_big_end_clear), (14 bytes).
    Removing norflash.o(i.norflash_big_end_enable), (20 bytes).
    Removing norflash.o(i.norflash_check_crc32), (14 bytes).
    Removing norflash.o(i.norflash_check_id), (72 bytes).
    Removing norflash.o(i.norflash_dma_callback), (24 bytes).
    Removing norflash.o(i.norflash_dma_read), (156 bytes).
    Removing norflash.o(i.norflash_dma_write), (252 bytes).
    Removing norflash.o(i.norflash_dual_read), (60 bytes).
    Removing norflash.o(i.norflash_dual_write), (112 bytes).
    Removing norflash.o(i.norflash_en4b), (40 bytes).
    Removing norflash.o(i.norflash_en_quad), (116 bytes).
    Removing norflash.o(i.norflash_en_quad_check), (64 bytes).
    Removing norflash.o(i.norflash_erase_block), (44 bytes).
    Removing norflash.o(i.norflash_erase_chip), (28 bytes).
    Removing norflash.o(i.norflash_erase_sector), (44 bytes).
    Removing norflash.o(i.norflash_ex4b), (40 bytes).
    Removing norflash.o(i.norflash_exit_quad), (76 bytes).
    Removing norflash.o(i.norflash_get_dual_hstatus), (52 bytes).
    Removing norflash.o(i.norflash_get_hstatus), (52 bytes).
    Removing norflash.o(i.norflash_get_status), (52 bytes).
    Removing norflash.o(i.norflash_init), (48 bytes).
    Removing norflash.o(i.norflash_quad_read), (76 bytes).
    Removing norflash.o(i.norflash_quad_write), (108 bytes).
    Removing norflash.o(i.norflash_read), (28 bytes).
    Removing norflash.o(i.norflash_read_config_reg), (36 bytes).
    Removing norflash.o(i.norflash_read_id), (20 bytes).
    Removing norflash.o(i.norflash_reset), (2 bytes).
    Removing norflash.o(i.norflash_reset_crc32), (32 bytes).
    Removing norflash.o(i.norflash_set_best_cfg), (50 bytes).
    Removing norflash.o(i.norflash_set_best_read_cfg), (84 bytes).
    Removing norflash.o(i.norflash_set_best_write_cfg), (84 bytes).
    Removing norflash.o(i.norflash_switch_fls_spi), (112 bytes).
    Removing norflash.o(i.norflash_write), (96 bytes).
    Removing norflash.o(i.norflash_write_disable), (64 bytes).
    Removing norflash.o(i.norflash_write_enable), (56 bytes).
    Removing norflash.o(i.norflash_write_endian_scr), (132 bytes).
    Removing norflash.o(.bss), (412 bytes).
    Removing norflash.o(.bss), (32 bytes).
    Removing norflash.o(.data), (2 bytes).
    Removing drv_common.o(.rev16_text), (4 bytes).
    Removing drv_common.o(.revsh_text), (4 bytes).
    Removing drv_common.o(i.drv_common_disable_systick), (20 bytes).
    Removing drv_common.o(i.drv_common_get_tick), (12 bytes).
    Removing drv_common.o(i.drv_common_idle_mode), (40 bytes).
    Removing drv_common.o(i.drv_common_systick_register_cb), (12 bytes).
    Removing drv_crgu.o(.rev16_text), (4 bytes).
    Removing drv_crgu.o(.revsh_text), (4 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_all_reset_flags), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_reset_flag), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_config_clocks), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_config_clocks_div), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_config_clocks_src), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_ana_clk_status), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_fpga_id), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_mipi_ref_src), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_reset_flag), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_system_clk), (28 bytes).
    Removing drv_crgu.o(i.drv_crgu_reset_chip), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_200m_scan_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_300m_scan_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_abp0_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_adc_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_adc_src), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_apb1_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_apb2_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_fls_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_fls_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_monitor_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_monitor_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_swire_div), (20 bytes).
    Removing drv_dma.o(.rev16_text), (4 bytes).
    Removing drv_dma.o(.revsh_text), (4 bytes).
    Removing drv_dma.o(i.drv_dma_abort_transfer), (32 bytes).
    Removing drv_dma.o(i.drv_dma_ahb_init), (74 bytes).
    Removing drv_dma.o(i.drv_dma_channel_is_active), (20 bytes).
    Removing drv_dma.o(i.drv_dma_deinit), (32 bytes).
    Removing drv_dma.o(i.drv_dma_disenable_channel_interrupts), (24 bytes).
    Removing drv_dma.o(i.drv_dma_enable_cycle), (44 bytes).
    Removing drv_dma.o(i.drv_dma_get_remaining_bytes), (32 bytes).
    Removing drv_dma.o(i.drv_dma_init), (24 bytes).
    Removing drv_dma.o(i.drv_dma_m2m_init), (72 bytes).
    Removing drv_dma.o(i.drv_dma_reset), (10 bytes).
    Removing drv_dma.o(i.drv_dma_set_ccr), (114 bytes).
    Removing drv_dma.o(i.drv_dma_start_transfer), (32 bytes).
    Removing drv_fls.o(.rev16_text), (4 bytes).
    Removing drv_fls.o(.revsh_text), (4 bytes).
    Removing drv_fls.o(i.__NVIC_DisableIRQ), (32 bytes).
    Removing drv_fls.o(i.drv_fls_gpio_connect), (28 bytes).
    Removing drv_fls.o(i.drv_fls_gpio_disconnect), (32 bytes).
    Removing drv_fls.o(i.fls_EnableClk), (12 bytes).
    Removing drv_fls.o(i.fls_busy_pending), (12 bytes).
    Removing drv_fls.o(i.fls_clear_irq_status), (6 bytes).
    Removing drv_fls.o(i.fls_ctrl_cfg_init), (72 bytes).
    Removing drv_fls.o(i.fls_ddat_enable), (24 bytes).
    Removing drv_fls.o(i.fls_de_init), (52 bytes).
    Removing drv_fls.o(i.fls_descr), (10 bytes).
    Removing drv_fls.o(i.fls_disable_it), (36 bytes).
    Removing drv_fls.o(i.fls_en_scr), (10 bytes).
    Removing drv_fls.o(i.fls_enable_it), (48 bytes).
    Removing drv_fls.o(i.fls_get_crcout), (4 bytes).
    Removing drv_fls.o(i.fls_get_default_fls_config), (20 bytes).
    Removing drv_fls.o(i.fls_get_default_spi_config), (44 bytes).
    Removing drv_fls.o(i.fls_get_default_tuning), (12 bytes).
    Removing drv_fls.o(i.fls_get_tuning), (18 bytes).
    Removing drv_fls.o(i.fls_init), (62 bytes).
    Removing drv_fls.o(i.fls_qadr_enable), (22 bytes).
    Removing drv_fls.o(i.fls_qcmd_enable), (22 bytes).
    Removing drv_fls.o(i.fls_qdat_enable), (22 bytes).
    Removing drv_fls.o(i.fls_read_byte_data), (130 bytes).
    Removing drv_fls.o(i.fls_read_cmd), (104 bytes).
    Removing drv_fls.o(i.fls_read_cmd_it), (110 bytes).
    Removing drv_fls.o(i.fls_reset_crc), (18 bytes).
    Removing drv_fls.o(i.fls_scr_clear), (10 bytes).
    Removing drv_fls.o(i.fls_set_addr_dummy), (32 bytes).
    Removing drv_fls.o(i.fls_set_addr_len), (32 bytes).
    Removing drv_fls.o(i.fls_set_mc_irq_mask), (26 bytes).
    Removing drv_fls.o(i.fls_set_read), (10 bytes).
    Removing drv_fls.o(i.fls_set_tuning), (24 bytes).
    Removing drv_fls.o(i.fls_set_write), (10 bytes).
    Removing drv_fls.o(i.fls_single_mode), (16 bytes).
    Removing drv_fls.o(i.fls_spi_init), (180 bytes).
    Removing drv_fls.o(i.fls_spi_start), (10 bytes).
    Removing drv_fls.o(i.fls_swrst), (18 bytes).
    Removing drv_fls.o(i.fls_write_byte_data), (164 bytes).
    Removing drv_fls.o(i.fls_write_cmd), (58 bytes).
    Removing drv_fls.o(.data), (4 bytes).
    Removing drv_gpio.o(.rev16_text), (4 bytes).
    Removing drv_gpio.o(.revsh_text), (4 bytes).
    Removing drv_gpio.o(i.drv_gpio_get_pull_state), (224 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_driving_strength), (312 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_schmitt_trigger), (168 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_slew_rate), (168 bytes).
    Removing drv_i2c_dma.o(.rev16_text), (4 bytes).
    Removing drv_i2c_dma.o(.revsh_text), (4 bytes).
    Removing drv_i2c_master.o(.rev16_text), (4 bytes).
    Removing drv_i2c_master.o(.revsh_text), (4 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_bus_init), (36 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_disable_intr), (16 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_get_fifo_status), (28 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_read_data), (32 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_set_fifo_threshold), (24 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_set_sys_mask), (48 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_write_data), (32 bytes).
    Removing drv_i2c_slave.o(.rev16_text), (4 bytes).
    Removing drv_i2c_slave.o(.revsh_text), (4 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_bus_init), (36 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_disable_intr), (16 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_enable), (16 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_get_tx_byte_num), (12 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_read_data), (32 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_set_fifo_threshold), (24 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_set_sys_mask), (48 bytes).
    Removing drv_param_init.o(.rev16_text), (4 bytes).
    Removing drv_param_init.o(.revsh_text), (4 bytes).
    Removing drv_param_init.o(i.drv_param_init_set_sclu_filter), (28 bytes).
    Removing drv_pwr.o(.rev16_text), (4 bytes).
    Removing drv_pwr.o(.revsh_text), (4 bytes).
    Removing drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode), (44 bytes).
    Removing drv_spi_dma.o(.rev16_text), (4 bytes).
    Removing drv_spi_dma.o(.revsh_text), (4 bytes).
    Removing drv_spi_dma.o(i.__NVIC_ClearPendingIRQ), (24 bytes).
    Removing drv_spi_dma.o(i.drv_spi_abort_dma), (108 bytes).
    Removing drv_spi_dma.o(i.drv_spi_dma_callback), (60 bytes).
    Removing drv_spi_dma.o(i.drv_spi_dma_ch6_init), (208 bytes).
    Removing drv_spi_dma.o(i.drv_spi_dma_init), (220 bytes).
    Removing drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback), (48 bytes).
    Removing drv_spi_dma.o(i.drv_spi_set_dma_irq_callback), (88 bytes).
    Removing drv_spi_dma.o(i.drv_spim_dma_read), (96 bytes).
    Removing drv_spi_dma.o(i.drv_spim_dma_write), (60 bytes).
    Removing drv_spi_dma.o(i.drv_spis_dma_write), (72 bytes).
    Removing drv_spi_dma.o(.bss), (480 bytes).
    Removing drv_spi_dma.o(.data), (16 bytes).
    Removing drv_spi_master.o(.rev16_text), (4 bytes).
    Removing drv_spi_master.o(.revsh_text), (4 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_deinit), (40 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_disable_int), (68 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_enable_int), (72 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_enable_rx_dma), (32 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_enable_tx_dma), (28 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_get_dma_address), (8 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_gpio_init), (32 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_set_intr_callback), (12 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_switch_sclk), (28 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_write_data), (44 bytes).
    Removing drv_spi_master.o(i.drv_spi_master_init), (164 bytes).
    Removing drv_sys_cfg.o(.rev16_text), (4 bytes).
    Removing drv_sys_cfg.o(.revsh_text), (4 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_dma_req_mask), (32 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_read_version0_id), (12 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_set_ap_reset), (28 bytes).
    Removing drv_timer.o(.rev16_text), (4 bytes).
    Removing drv_timer.o(.revsh_text), (4 bytes).
    Removing drv_timer.o(i.drv_timer_clean_timer_value), (12 bytes).
    Removing drv_timer.o(i.drv_timer_get_current_count), (10 bytes).
    Removing drv_timer.o(i.drv_timer_get_match), (10 bytes).
    Removing drv_timer.o(i.drv_timer_set_repeat), (16 bytes).
    Removing hal_internal_vsync.o(.rev16_text), (4 bytes).
    Removing hal_internal_vsync.o(.revsh_text), (4 bytes).
    Removing hal_internal_vsync.o(i.hal_iniernal_vsync_deinit), (20 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual), (528 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode), (48 bytes).
    Removing dcs_packet_fifo.o(i.dcs_packet_get_fifo_size), (16 bytes).
    Removing drv_dsi_rx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_rx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate), (66 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_version), (4 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration), (236 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg), (32 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg), (48 bytes).
    Removing drv_dsi_rx.o(i.drv_rx_phy_test_read), (12 bytes).
    Removing drv_dsi_tx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_tx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_force_interrupt), (8 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_get_phy_status), (6 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_forcepll), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration), (232 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_start), (18 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock), (10 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot), (62 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger), (92 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter), (344 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit), (276 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_sdf_3d), (28 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_bta), (22 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_vpg), (70 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_version), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_vid_shadow), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_read), (10 bytes).
    Removing drv_lcdc.o(.rev16_text), (4 bytes).
    Removing drv_lcdc.o(.revsh_text), (4 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_config_rgb_to_pentile), (26 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_enable), (42 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_set_prefetch), (24 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_update_shadow_reg), (12 bytes).
    Removing drv_memc.o(.rev16_text), (4 bytes).
    Removing drv_memc.o(.revsh_text), (4 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_frm_time), (14 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_int_frame), (28 bytes).
    Removing drv_memc.o(i.drv_memc_set_fb_remaining_line_trigger), (12 bytes).
    Removing drv_memc.o(i.drv_memc_set_read_trigger_line), (16 bytes).
    Removing drv_memc.o(i.drv_memc_set_te_ind), (16 bytes).
    Removing drv_memc.o(i.drv_memc_set_tear_hwclr), (16 bytes).
    Removing drv_memc.o(i.drv_memc_set_vidc_fb_arb), (14 bytes).
    Removing drv_memc.o(i.drv_memc_set_write_trigger_line), (16 bytes).
    Removing drv_rxbr.o(.rev16_text), (4 bytes).
    Removing drv_rxbr.o(.revsh_text), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_dsc_flush), (16 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_cur_hline_rcv_cnt), (8 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_ipi_vsync_interval), (8 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_pix_fmt), (8 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_col_addr), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_compress), (24 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_page_addr), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_soft_reset), (98 bytes).
    Removing drv_vidc.o(.rev16_text), (4 bytes).
    Removing drv_vidc.o(.revsh_text), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_clear_status0), (14 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_cap_pixel), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_signal_frame), (30 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_int_source), (38 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status0), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status1), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status2), (6 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_dsc_thresh), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_frmst_latency), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_inff_thresh), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_irq_line), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_module_enable), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_outff_thresh), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_update_src_format), (14 bytes).
    Removing irq_redirect .o(.rev16_text), (4 bytes).
    Removing irq_redirect .o(.revsh_text), (4 bytes).
    Removing drv_phy_common.o(.rev16_text), (4 bytes).
    Removing drv_phy_common.o(.revsh_text), (4 bytes).
    Removing drv_phy_common.o(i.drv_phy_test_read), (8 bytes).
    Removing drv_chip_info.o(.rev16_text), (4 bytes).
    Removing drv_chip_info.o(.revsh_text), (4 bytes).
    Removing drv_dsc_dec.o(.rev16_text), (4 bytes).
    Removing drv_dsc_dec.o(.revsh_text), (4 bytes).
    Removing drv_dsc_dec.o(i.drv_dsc_dec_set_u32_pps), (120 bytes).
    Removing hal_spi_slave.o(.rev16_text), (4 bytes).
    Removing hal_spi_slave.o(.revsh_text), (4 bytes).
    Removing hal_spi_slave.o(i.hal_spi_s_set_high_impedance), (100 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_auto_transfer_abort), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start), (56 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_busy), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_deinit), (10 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_disable), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_enable), (96 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_flush_fifo), (20 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_get_rxfifo_notempty), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_gpio_init), (8 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_init), (76 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_read_data), (10 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_register_callback), (12 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_reset_tx), (68 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_set_auto_rx_buffer), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_set_auto_tx_buffer), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_write_data), (14 bytes).
    Removing drv_fls_dma.o(.rev16_text), (4 bytes).
    Removing drv_fls_dma.o(.revsh_text), (4 bytes).
    Removing drv_fls_dma.o(i.fls_abort_dma), (42 bytes).
    Removing drv_fls_dma.o(i.fls_dma_disable), (10 bytes).
    Removing drv_fls_dma.o(i.fls_dma_enable), (10 bytes).
    Removing drv_fls_dma.o(i.fls_dma_read_prepare), (86 bytes).
    Removing drv_fls_dma.o(i.fls_dma_write_prepare), (82 bytes).
    Removing drv_fls_dma.o(i.fls_read_dmacallback), (32 bytes).
    Removing drv_fls_dma.o(i.fls_transfer_create_handle_dma), (208 bytes).
    Removing drv_fls_dma.o(i.fls_transfer_dma), (112 bytes).
    Removing drv_fls_dma.o(i.fls_transfer_get_receive_count_dma), (44 bytes).
    Removing drv_fls_dma.o(i.fls_write_dmacallback), (32 bytes).
    Removing drv_fls_dma.o(.data), (8 bytes).
    Removing drv_pwm.o(.rev16_text), (4 bytes).
    Removing drv_pwm.o(.revsh_text), (4 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_clear_pwm_int_all), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_enable), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_counter_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_current_count), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_high_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_low_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_register_callback), (24 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_set_pwm_int), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_set_sys_int), (52 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_enable), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_get_sync_flag), (16 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_pause), (28 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_control), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_sync_mode), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_threshold), (12 bytes).
    Removing drv_spi_slave.o(.rev16_text), (4 bytes).
    Removing drv_spi_slave.o(.revsh_text), (4 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_deinit), (40 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_disable_int), (68 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_enable_int), (72 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_enable_rx_dma), (32 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_enable_tx_dma), (28 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_get_dma_address), (8 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_gpio_init), (24 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_read_data), (32 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_switch_sclk), (28 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_write_data), (44 bytes).
    Removing drv_spi_slave.o(i.drv_spi_slave_init), (76 bytes).
    Removing drv_swire.o(.rev16_text), (4 bytes).
    Removing drv_swire.o(.revsh_text), (4 bytes).
    Removing drv_swire.o(i.drv_swire_enable), (28 bytes).
    Removing drv_swire.o(i.drv_swire_register_callback), (12 bytes).
    Removing drv_swire.o(i.drv_swire_set_bit_time), (24 bytes).
    Removing drv_swire.o(i.drv_swire_set_power_down), (28 bytes).
    Removing drv_swire.o(i.drv_swire_set_pulse_count), (12 bytes).
    Removing drv_uart.o(.rev16_text), (4 bytes).
    Removing drv_uart.o(.revsh_text), (4 bytes).
    Removing drv_uart.o(i.UART_AbortReceive), (30 bytes).
    Removing drv_uart.o(i.UART_AbortSend), (30 bytes).
    Removing drv_uart.o(i.UART_Deinit), (28 bytes).
    Removing drv_uart.o(i.UART_Disable_IT), (68 bytes).
    Removing drv_uart.o(i.UART_EnableDma), (32 bytes).
    Removing drv_uart.o(i.UART_Enable_IT), (44 bytes).
    Removing drv_uart.o(i.UART_GetDefaultConfig), (72 bytes).
    Removing drv_uart.o(i.UART_GetFIFO_Ctrl), (20 bytes).
    Removing drv_uart.o(i.UART_GetReceiveCount), (22 bytes).
    Removing drv_uart.o(i.UART_GetReceiveStatus), (20 bytes).
    Removing drv_uart.o(i.UART_GetRxRingBufferLength), (28 bytes).
    Removing drv_uart.o(i.UART_GetSendCount), (22 bytes).
    Removing drv_uart.o(i.UART_GetSendStatus), (20 bytes).
    Removing drv_uart.o(i.UART_ReadBlocking), (32 bytes).
    Removing drv_uart.o(i.UART_ReceiveNonBlocking), (50 bytes).
    Removing drv_uart.o(i.UART_ResetTxFIFO), (36 bytes).
    Removing drv_uart.o(i.UART_SendNonBlocking), (38 bytes).
    Removing drv_uart.o(i.UART_TransferCreateHandle), (96 bytes).
    Removing drv_uart.o(i.UART_TransferStartRingBuffer), (30 bytes).
    Removing drv_uart.o(.constdata), (1 bytes).
    Removing drv_uart_dma.o(.rev16_text), (4 bytes).
    Removing drv_uart_dma.o(.revsh_text), (4 bytes).
    Removing drv_uart_dma.o(i.UART_DMAInit), (76 bytes).
    Removing drv_uart_dma.o(i.UART_TransferAbortReceiveDMA), (16 bytes).
    Removing drv_uart_dma.o(i.UART_TransferAbortSendDMA), (16 bytes).
    Removing drv_uart_dma.o(i.UART_TransferCreateHandleDMA), (176 bytes).
    Removing drv_uart_dma.o(i.UART_TransferGetReceiveCountDMA), (44 bytes).
    Removing drv_uart_dma.o(i.UART_TransferReceiveDMA), (68 bytes).
    Removing drv_uart_dma.o(i.UART_TransferReceiveDMACallback), (34 bytes).
    Removing drv_uart_dma.o(i.UART_TransferSendDMA), (68 bytes).
    Removing drv_uart_dma.o(i.UART_TransferSendDMACallback), (34 bytes).
    Removing drv_uart_dma.o(.data), (8 bytes).
    Removing drv_wdg.o(.rev16_text), (4 bytes).
    Removing drv_wdg.o(.revsh_text), (4 bytes).
    Removing drv_wdg.o(i.drv_wdg_enable), (32 bytes).
    Removing drv_wdg.o(i.drv_wdg_load_match), (12 bytes).
    Removing drv_wdg.o(i.drv_wdg_register_callback), (12 bytes).
    Removing drv_wdg.o(i.drv_wdg_sel_mode), (28 bytes).
    Removing drv_wdg.o(i.drv_wdg_set_repeat), (12 bytes).
    Removing drv_efuse.o(.rev16_text), (4 bytes).
    Removing drv_efuse.o(.revsh_text), (4 bytes).
    Removing drv_efuse.o(i.drv_efuse_crc_cal), (128 bytes).
    Removing drv_efuse.o(i.drv_efuse_get_default_config), (26 bytes).
    Removing drv_efuse.o(i.drv_efuse_int_disable), (12 bytes).
    Removing drv_efuse.o(i.drv_efuse_write), (46 bytes).
    Removing drv_efuse.o(i.drv_efuse_write_req), (22 bytes).
    Removing dflti.o(.text), (40 bytes).

575 unused section(s) (total 26123 bytes) removed from the image.

==============================================================================

Image Symbol Table

    Local Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    ../clib/../cmprslib/zerorunl2.c          0x00000000   Number         0  __dczerorl2.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  idiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uidiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uldiv.o ABSOLUTE
    ../clib/microlib/errno.c                 0x00000000   Number         0  errno.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry2.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry5.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11a.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llshl.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llushr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llsshr.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf5.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf8.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf7.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf6.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf4.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfa.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf3.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf2.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf1.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf0.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfb.o ABSOLUTE
    ../clib/microlib/printf/stubs.s          0x00000000   Number         0  stubs.o ABSOLUTE
    ../clib/microlib/stdio/streams.c         0x00000000   Number         0  stdout.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpyb.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpya.o ABSOLUTE
    ../clib/microlib/string/memset.c         0x00000000   Number         0  memseta.o ABSOLUTE
    ../clib/microlib/stubs.s                 0x00000000   Number         0  iusefp.o ABSOLUTE
    ../fplib/microlib/f2d.c                  0x00000000   Number         0  f2d.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  dadd.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  fadd.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  ddiv.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  fdiv.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  fepilogue.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  depilogue.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixi.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixul.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  ffixi.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  ffixui.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixui.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  ffltui.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  dflti.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  dfltui.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  fflti.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  fmul.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  dmul.o ABSOLUTE
    ../fplib/microlib/fpscalb.c              0x00000000   Number         0  fscalb.o ABSOLUTE
    ../fplib/microlib/fpsqrt.c               0x00000000   Number         0  dsqrt.o ABSOLUTE
    ../mathlib/ceil.c                        0x00000000   Number         0  ceil.o ABSOLUTE
    ../mathlib/sqrt.c                        0x00000000   Number         0  sqrt_x.o ABSOLUTE
    ../mathlib/sqrt.c                        0x00000000   Number         0  sqrt.o ABSOLUTE
    ..\..\..\src\common\tau_delay.c          0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\..\..\src\common\tau_log.c            0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\..\..\src\driver\robin\src\drv_chip_info.c 0x00000000   Number         0  drv_chip_info.o ABSOLUTE
    ..\..\..\src\driver\robin\src\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\irq_redirect .c 0x00000000   Number         0  irq_redirect .o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\internal\dcs_packet_fifo.c 0x00000000   Number         0  dcs_packet_fifo.o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\internal\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_fls.c 0x00000000   Number         0  drv_fls.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_fls_dma.c 0x00000000   Number         0  drv_fls_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_i2c_dma.c 0x00000000   Number         0  drv_i2c_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_i2c_master.c 0x00000000   Number         0  drv_i2c_master.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_i2c_slave.c 0x00000000   Number         0  drv_i2c_slave.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_param_init.c 0x00000000   Number         0  drv_param_init.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_pwm.c 0x00000000   Number         0  drv_pwm.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_spi_dma.c 0x00000000   Number         0  drv_spi_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_spi_master.c 0x00000000   Number         0  drv_spi_master.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_spi_slave.c 0x00000000   Number         0  drv_spi_slave.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_uart_dma.c 0x00000000   Number         0  drv_uart_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_wdg.c 0x00000000   Number         0  drv_wdg.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_i2c_master.c 0x00000000   Number         0  hal_i2c_master.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_i2c_slave.c 0x00000000   Number         0  hal_i2c_slave.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_spi_master.c 0x00000000   Number         0  hal_spi_master.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_spi_slave.c 0x00000000   Number         0  hal_spi_slave.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_timer.c 0x00000000   Number         0  hal_timer.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\internal\norflash.c 0x00000000   Number         0  norflash.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_delay.c     0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_log.c       0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\\..\\..\\src\\driver\\robin\\src\\drv_chip_info.c 0x00000000   Number         0  drv_chip_info.o ABSOLUTE
    ..\\..\\..\\src\\driver\\robin\\src\\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\irq_redirect .c 0x00000000   Number         0  irq_redirect .o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\hal\\internal\\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_fls.c 0x00000000   Number         0  drv_fls.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_fls_dma.c 0x00000000   Number         0  drv_fls_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_i2c_dma.c 0x00000000   Number         0  drv_i2c_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_i2c_master.c 0x00000000   Number         0  drv_i2c_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_i2c_slave.c 0x00000000   Number         0  drv_i2c_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_param_init.c 0x00000000   Number         0  drv_param_init.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_pwm.c 0x00000000   Number         0  drv_pwm.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_spi_dma.c 0x00000000   Number         0  drv_spi_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_spi_master.c 0x00000000   Number         0  drv_spi_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_spi_slave.c 0x00000000   Number         0  drv_spi_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_uart_dma.c 0x00000000   Number         0  drv_uart_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_wdg.c 0x00000000   Number         0  drv_wdg.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_i2c_master.c 0x00000000   Number         0  hal_i2c_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_i2c_slave.c 0x00000000   Number         0  hal_i2c_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_spi_master.c 0x00000000   Number         0  hal_spi_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_spi_slave.c 0x00000000   Number         0  hal_spi_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_timer.c 0x00000000   Number         0  hal_timer.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\internal\\norflash.c 0x00000000   Number         0  norflash.o ABSOLUTE
    ..\\src\\app\\demo\\ap_demo.c            0x00000000   Number         0  ap_demo.o ABSOLUTE
    ..\\src\\app\\demo\\app_tp_for_custom_s8.c 0x00000000   Number         0  app_tp_for_custom_s8.o ABSOLUTE
    ..\\src\\app\\demo\\app_tp_st_touch.c    0x00000000   Number         0  app_tp_st_touch.o ABSOLUTE
    ..\\src\\app\\demo\\app_tp_transfer.c    0x00000000   Number         0  app_tp_transfer.o ABSOLUTE
    ..\\src\\app\\main.c                     0x00000000   Number         0  main.o ABSOLUTE
    ..\\src\\board\\board.c                  0x00000000   Number         0  board.o ABSOLUTE
    ..\src\app\demo\ap_demo.c                0x00000000   Number         0  ap_demo.o ABSOLUTE
    ..\src\app\demo\app_tp_for_custom_s8.c   0x00000000   Number         0  app_tp_for_custom_s8.o ABSOLUTE
    ..\src\app\demo\app_tp_st_touch.c        0x00000000   Number         0  app_tp_st_touch.o ABSOLUTE
    ..\src\app\demo\app_tp_transfer.c        0x00000000   Number         0  app_tp_transfer.o ABSOLUTE
    ..\src\app\main.c                        0x00000000   Number         0  main.o ABSOLUTE
    ..\src\board\board.c                     0x00000000   Number         0  board.o ABSOLUTE
    ..\src\board\startup\startup_ARMCM0.s    0x00000000   Number         0  startup_armcm0.o ABSOLUTE
    cdcmple.s                                0x00000000   Number         0  cdcmple.o ABSOLUTE
    cdrcmple.s                               0x00000000   Number         0  cdrcmple.o ABSOLUTE
    cfrcmple.s                               0x00000000   Number         0  cfrcmple.o ABSOLUTE
    dc.s                                     0x00000000   Number         0  dc.o ABSOLUTE
    handlers.s                               0x00000000   Number         0  handlers.o ABSOLUTE
    init.s                                   0x00000000   Number         0  init.o ABSOLUTE
    RESET                                    0x00010000   Section      192  startup_armcm0.o(RESET)
    .ARM.Collect$$$$00000000                 0x000100c0   Section        0  entry.o(.ARM.Collect$$$$00000000)
    .ARM.Collect$$$$00000001                 0x000100c0   Section        4  entry2.o(.ARM.Collect$$$$00000001)
    .ARM.Collect$$$$00000004                 0x000100c4   Section        4  entry5.o(.ARM.Collect$$$$00000004)
    .ARM.Collect$$$$00000008                 0x000100c8   Section        0  entry7b.o(.ARM.Collect$$$$00000008)
    .ARM.Collect$$$$0000000A                 0x000100c8   Section        0  entry8b.o(.ARM.Collect$$$$0000000A)
    .ARM.Collect$$$$0000000B                 0x000100c8   Section        8  entry9a.o(.ARM.Collect$$$$0000000B)
    .ARM.Collect$$$$0000000D                 0x000100d0   Section        0  entry10a.o(.ARM.Collect$$$$0000000D)
    .ARM.Collect$$$$0000000F                 0x000100d0   Section        0  entry11a.o(.ARM.Collect$$$$0000000F)
    .ARM.Collect$$$$00002712                 0x000100d0   Section        4  entry2.o(.ARM.Collect$$$$00002712)
    __lit__00000000                          0x000100d0   Data           4  entry2.o(.ARM.Collect$$$$00002712)
    .text                                    0x000100d4   Section      120  startup_armcm0.o(.text)
    .text                                    0x0001014c   Section        0  uidiv.o(.text)
    .text                                    0x00010178   Section        0  idiv.o(.text)
    .text                                    0x000101a0   Section        0  memcpya.o(.text)
    .text                                    0x000101c4   Section        0  memseta.o(.text)
    .text                                    0x000101e8   Section        0  fadd.o(.text)
    .text                                    0x0001029a   Section        0  fmul.o(.text)
    .text                                    0x00010314   Section        0  fdiv.o(.text)
    .text                                    0x00010390   Section        0  fscalb.o(.text)
    .text                                    0x000103a8   Section        0  dadd.o(.text)
    .text                                    0x0001050c   Section        0  dmul.o(.text)
    .text                                    0x000105dc   Section        0  ddiv.o(.text)
    .text                                    0x000106cc   Section        0  fflti.o(.text)
    .text                                    0x000106e2   Section        0  ffltui.o(.text)
    .text                                    0x000106f0   Section        0  dfltui.o(.text)
    .text                                    0x0001070c   Section        0  ffixi.o(.text)
    .text                                    0x0001073e   Section        0  ffixui.o(.text)
    .text                                    0x00010768   Section        0  dfixi.o(.text)
    .text                                    0x000107b0   Section        0  dfixui.o(.text)
    .text                                    0x000107ec   Section        0  f2d.o(.text)
    .text                                    0x00010814   Section       40  cdcmple.o(.text)
    .text                                    0x0001083c   Section       20  cfrcmple.o(.text)
    .text                                    0x00010850   Section        0  uldiv.o(.text)
    .text                                    0x000108b0   Section        0  llshl.o(.text)
    .text                                    0x000108d0   Section        0  llushr.o(.text)
    .text                                    0x000108f2   Section        0  llsshr.o(.text)
    .text                                    0x00010918   Section        0  fepilogue.o(.text)
    .text                                    0x00010918   Section        0  iusefp.o(.text)
    .text                                    0x0001099a   Section        0  depilogue.o(.text)
    .text                                    0x00010a58   Section        0  dsqrt.o(.text)
    .text                                    0x00010afc   Section        0  dfixul.o(.text)
    .text                                    0x00010b3c   Section       40  cdrcmple.o(.text)
    .text                                    0x00010b64   Section       36  init.o(.text)
    .text                                    0x00010b88   Section        0  __dczerorl2.o(.text)
    i.ADC_IRQn_Handler                       0x00010be0   Section        0  irq_redirect .o(i.ADC_IRQn_Handler)
    i.AP_NRESET_IRQn_Handler                 0x00010bf8   Section        0  irq_redirect .o(i.AP_NRESET_IRQn_Handler)
    i.CRC16_2                                0x00010c10   Section        0  app_tp_st_touch.o(i.CRC16_2)
    i.DMA_IRQn_Handler                       0x00010c50   Section        0  irq_redirect .o(i.DMA_IRQn_Handler)
    i.EXTI_INT0_IRQn_Handler                 0x00010c64   Section        0  irq_redirect .o(i.EXTI_INT0_IRQn_Handler)
    i.EXTI_INT1_IRQn_Handler                 0x00010c80   Section        0  irq_redirect .o(i.EXTI_INT1_IRQn_Handler)
    i.EXTI_INT2_IRQn_Handler                 0x00010c9c   Section        0  irq_redirect .o(i.EXTI_INT2_IRQn_Handler)
    i.EXTI_INT3_IRQn_Handler                 0x00010cb8   Section        0  irq_redirect .o(i.EXTI_INT3_IRQn_Handler)
    i.EXTI_INT4_IRQn_Handler                 0x00010cd4   Section        0  irq_redirect .o(i.EXTI_INT4_IRQn_Handler)
    i.EXTI_INT5_IRQn_Handler                 0x00010cf0   Section        0  irq_redirect .o(i.EXTI_INT5_IRQn_Handler)
    i.EXTI_INT6_IRQn_Handler                 0x00010d0c   Section        0  irq_redirect .o(i.EXTI_INT6_IRQn_Handler)
    i.EXTI_INT7_IRQn_Handler                 0x00010d28   Section        0  irq_redirect .o(i.EXTI_INT7_IRQn_Handler)
    i.FLSCTRL_IRQn_Handler                   0x00010d44   Section        0  irq_redirect .o(i.FLSCTRL_IRQn_Handler)
    i.Gpio_swire_output                      0x00010d58   Section        0  ap_demo.o(i.Gpio_swire_output)
    i.HardFault_Handler                      0x00010da8   Section        0  irq_redirect .o(i.HardFault_Handler)
    i.I2C0_IRQn_Handler                      0x00010dbc   Section        0  irq_redirect .o(i.I2C0_IRQn_Handler)
    i.I2C1_IRQn_Handler                      0x00010dd4   Section        0  irq_redirect .o(i.I2C1_IRQn_Handler)
    i.LCDC_IRQn_Handler                      0x00010dec   Section        0  irq_redirect .o(i.LCDC_IRQn_Handler)
    i.LOG_printf                             0x00010e04   Section        0  tau_log.o(i.LOG_printf)
    i.MEMC_IRQn_Handler                      0x00010e2c   Section        0  irq_redirect .o(i.MEMC_IRQn_Handler)
    i.MIPI_RX_IRQn_Handler                   0x00010e44   Section        0  irq_redirect .o(i.MIPI_RX_IRQn_Handler)
    i.MIPI_TX_IRQn_Handler                   0x00010e5c   Section        0  irq_redirect .o(i.MIPI_TX_IRQn_Handler)
    i.PWMDET_IRQn_Handler                    0x00010e74   Section        0  irq_redirect .o(i.PWMDET_IRQn_Handler)
    i.S20_Start_init                         0x00010e90   Section        0  app_tp_transfer.o(i.S20_Start_init)
    i.SPIM_IRQn_Handler                      0x00010fd4   Section        0  irq_redirect .o(i.SPIM_IRQn_Handler)
    i.UART_DisableDma                        0x00010ff0   Section        0  drv_uart.o(i.UART_DisableDma)
    i.UART_GetInstance                       0x00010ff2   Section        0  drv_uart.o(i.UART_GetInstance)
    i.__scatterload_null                     0x00010ff6   Section        2  handlers.o(i.__scatterload_null)
    i.app_UART_IRQn_Handler                  0x00010ff8   Section        0  drv_uart.o(i.app_UART_IRQn_Handler)
    .ARM.__at_0x11000                        0x00011000   Section       20  drv_common.o(.ARM.__at_0x11000)
    i.SPIS_IRQn_Handler                      0x00011014   Section        0  irq_redirect .o(i.SPIS_IRQn_Handler)
    i.SWIRE_IRQn_Handler                     0x00011030   Section        0  irq_redirect .o(i.SWIRE_IRQn_Handler)
    i.SysTick_Handler                        0x0001104c   Section        0  irq_redirect .o(i.SysTick_Handler)
    i.TIMER0_IRQn_Handler                    0x00011064   Section        0  irq_redirect .o(i.TIMER0_IRQn_Handler)
    i.TIMER1_IRQn_Handler                    0x0001107c   Section        0  irq_redirect .o(i.TIMER1_IRQn_Handler)
    i.TIMER2_IRQn_Handler                    0x00011094   Section        0  irq_redirect .o(i.TIMER2_IRQn_Handler)
    i.TIMER3_IRQn_Handler                    0x000110ac   Section        0  irq_redirect .o(i.TIMER3_IRQn_Handler)
    i.UART0_IRQ_Handle                       0x000110c4   Section        0  drv_uart.o(i.UART0_IRQ_Handle)
    i.UART_IRQn_Handler                      0x000110e0   Section        0  irq_redirect .o(i.UART_IRQn_Handler)
    i.UART_ResetRxFIFO                       0x000110f8   Section        0  drv_uart.o(i.UART_ResetRxFIFO)
    i.UART_SetBaudRate                       0x0001111c   Section        0  drv_uart.o(i.UART_SetBaudRate)
    i.UART_SwitchSCLK                        0x00011164   Section        0  drv_uart.o(i.UART_SwitchSCLK)
    i.UART_TransferHandleIRQ                 0x0001117e   Section        0  drv_uart.o(i.UART_TransferHandleIRQ)
    i.UART_WriteBlocking                     0x000112b2   Section        0  drv_uart.o(i.UART_WriteBlocking)
    i.UART_init                              0x000112cc   Section        0  drv_uart.o(i.UART_init)
    i.VIDC_IRQn_Handler                      0x00011388   Section        0  irq_redirect .o(i.VIDC_IRQn_Handler)
    i.VPRE_IRQn_Handler                      0x000113a0   Section        0  irq_redirect .o(i.VPRE_IRQn_Handler)
    i.WDG_IRQn_Handler                       0x000113b8   Section        0  irq_redirect .o(i.WDG_IRQn_Handler)
    i.__0printf                              0x000113d0   Section        0  printfa.o(i.__0printf)
    i.__0vsprintf                            0x000113f0   Section        0  printfa.o(i.__0vsprintf)
    i.__ARM_clz                              0x00011414   Section        0  depilogue.o(i.__ARM_clz)
    i.__ARM_common_switch8                   0x00011442   Section        0  hal_dsi_rx_ctrl.o(i.__ARM_common_switch8)
    i.__NVIC_ClearPendingIRQ                 0x0001145c   Section        0  drv_i2c_master.o(i.__NVIC_ClearPendingIRQ)
    __NVIC_ClearPendingIRQ                   0x0001145d   Thumb Code    18  drv_i2c_master.o(i.__NVIC_ClearPendingIRQ)
    i.__NVIC_ClearPendingIRQ                 0x00011474   Section        0  drv_i2c_slave.o(i.__NVIC_ClearPendingIRQ)
    __NVIC_ClearPendingIRQ                   0x00011475   Thumb Code    18  drv_i2c_slave.o(i.__NVIC_ClearPendingIRQ)
    i.__NVIC_ClearPendingIRQ                 0x0001148c   Section        0  drv_spi_master.o(i.__NVIC_ClearPendingIRQ)
    __NVIC_ClearPendingIRQ                   0x0001148d   Thumb Code    18  drv_spi_master.o(i.__NVIC_ClearPendingIRQ)
    i.__NVIC_DisableIRQ                      0x000114a4   Section        0  drv_rxbr.o(i.__NVIC_DisableIRQ)
    __NVIC_DisableIRQ                        0x000114a5   Thumb Code    26  drv_rxbr.o(i.__NVIC_DisableIRQ)
    i.__NVIC_EnableIRQ                       0x000114c4   Section        0  drv_rxbr.o(i.__NVIC_EnableIRQ)
    __NVIC_EnableIRQ                         0x000114c5   Thumb Code    18  drv_rxbr.o(i.__NVIC_EnableIRQ)
    i.__NVIC_SetPriority                     0x000114dc   Section        0  hal_spi_slave.o(i.__NVIC_SetPriority)
    __NVIC_SetPriority                       0x000114dd   Thumb Code    60  hal_spi_slave.o(i.__NVIC_SetPriority)
    i.__scatterload_copy                     0x00011520   Section       14  handlers.o(i.__scatterload_copy)
    i.__scatterload_zeroinit                 0x0001152e   Section       14  handlers.o(i.__scatterload_zeroinit)
    i.__set_errno                            0x0001153c   Section        0  errno.o(i.__set_errno)
    i._fp_digits                             0x00011548   Section        0  printfa.o(i._fp_digits)
    _fp_digits                               0x00011549   Thumb Code   344  printfa.o(i._fp_digits)
    i._printf_core                           0x000116bc   Section        0  printfa.o(i._printf_core)
    _printf_core                             0x000116bd   Thumb Code  1754  printfa.o(i._printf_core)
    i._printf_post_padding                   0x00011da8   Section        0  printfa.o(i._printf_post_padding)
    _printf_post_padding                     0x00011da9   Thumb Code    32  printfa.o(i._printf_post_padding)
    i._printf_pre_padding                    0x00011dc8   Section        0  printfa.o(i._printf_pre_padding)
    _printf_pre_padding                      0x00011dc9   Thumb Code    44  printfa.o(i._printf_pre_padding)
    i._sputc                                 0x00011df4   Section        0  printfa.o(i._sputc)
    _sputc                                   0x00011df5   Thumb Code    10  printfa.o(i._sputc)
    i.ap_dcs_read                            0x00011e00   Section        0  ap_demo.o(i.ap_dcs_read)
    ap_dcs_read                              0x00011e01   Thumb Code  4040  ap_demo.o(i.ap_dcs_read)
    i.ap_demo                                0x00012df4   Section        0  ap_demo.o(i.ap_demo)
    i.ap_get_reg_df                          0x00012f90   Section        0  ap_demo.o(i.ap_get_reg_df)
    ap_get_reg_df                            0x00012f91   Thumb Code   136  ap_demo.o(i.ap_get_reg_df)
    i.ap_get_tp_calibration_status_01        0x0001301c   Section        0  app_tp_st_touch.o(i.ap_get_tp_calibration_status_01)
    i.ap_reset_cb                            0x0001303c   Section        0  ap_demo.o(i.ap_reset_cb)
    ap_reset_cb                              0x0001303d   Thumb Code    42  ap_demo.o(i.ap_reset_cb)
    i.ap_set_backlight_51                    0x000130a4   Section        0  ap_demo.o(i.ap_set_backlight_51)
    ap_set_backlight_51                      0x000130a5   Thumb Code    28  ap_demo.o(i.ap_set_backlight_51)
    i.ap_set_display_off                     0x000130c0   Section        0  ap_demo.o(i.ap_set_display_off)
    ap_set_display_off                       0x000130c1   Thumb Code    28  ap_demo.o(i.ap_set_display_off)
    i.ap_set_display_on                      0x00013104   Section        0  ap_demo.o(i.ap_set_display_on)
    ap_set_display_on                        0x00013105   Thumb Code    16  ap_demo.o(i.ap_set_display_on)
    i.ap_set_enter_sleep_mode                0x0001313c   Section        0  ap_demo.o(i.ap_set_enter_sleep_mode)
    ap_set_enter_sleep_mode                  0x0001313d   Thumb Code    74  ap_demo.o(i.ap_set_enter_sleep_mode)
    i.ap_set_exit_sleep_mode                 0x000131b8   Section        0  ap_demo.o(i.ap_set_exit_sleep_mode)
    ap_set_exit_sleep_mode                   0x000131b9   Thumb Code    58  ap_demo.o(i.ap_set_exit_sleep_mode)
    i.ap_set_tp_calibration_04               0x00013228   Section        0  app_tp_st_touch.o(i.ap_set_tp_calibration_04)
    i.ap_tp_st_touch_calibration             0x000132c0   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_calibration)
    i.ap_tp_st_touch_error_handler_F3        0x00013370   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_F3)
    i.ap_tp_st_touch_error_handler_FF        0x0001338a   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_FF)
    i.ap_tp_st_touch_get_calibration_success_mark 0x000133ac   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark)
    i.ap_tp_st_touch_scan_point_init         0x00013454   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init)
    i.ap_tp_st_touch_scan_point_record_event 0x00013470   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event)
    i.ap_tp_st_touch_scan_point_record_event_exec 0x00013504   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec)
    i.ap_tp_st_touch_simulate_finger_release_event 0x00013554   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event)
    i.ap_tp_st_touch_software_reset          0x00013588   Section        0  app_tp_st_touch.o(i.ap_tp_st_touch_software_reset)
    i.ap_update_frame_rate                   0x00013634   Section        0  ap_demo.o(i.ap_update_frame_rate)
    ap_update_frame_rate                     0x00013635   Thumb Code    56  ap_demo.o(i.ap_update_frame_rate)
    i.app_ADC_IRQn_Handler                   0x000136a0   Section        0  drv_rxbr.o(i.app_ADC_IRQn_Handler)
    i.app_AP_NRESET_IRQn_Handler             0x000136bc   Section        0  drv_gpio.o(i.app_AP_NRESET_IRQn_Handler)
    i.app_EXTI_INT0_IRQn_Handler             0x000136e0   Section        0  drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler)
    i.app_EXTI_INT1_IRQn_Handler             0x000136fc   Section        0  drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler)
    i.app_EXTI_INT2_IRQn_Handler             0x00013718   Section        0  drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler)
    i.app_EXTI_INT3_IRQn_Handler             0x00013734   Section        0  drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler)
    i.app_EXTI_INT4_IRQn_Handler             0x00013750   Section        0  drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler)
    i.app_EXTI_INT5_IRQn_Handler             0x0001376c   Section        0  drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler)
    i.app_EXTI_INT6_IRQn_Handler             0x00013788   Section        0  drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler)
    i.app_EXTI_INT7_IRQn_Handler             0x000137a4   Section        0  drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler)
    i.app_HardFault_Handler                  0x000137c0   Section        0  drv_common.o(i.app_HardFault_Handler)
    i.app_I2C0_IRQn_Handler                  0x00013808   Section        0  drv_i2c_slave.o(i.app_I2C0_IRQn_Handler)
    i.app_I2C1_IRQn_Handler                  0x00013818   Section        0  drv_i2c_master.o(i.app_I2C1_IRQn_Handler)
    i.app_LCDC_IRQn_Handler                  0x00013828   Section        0  hal_internal_vsync.o(i.app_LCDC_IRQn_Handler)
    i.app_MEMC_IRQn_Handler                  0x00013908   Section        0  drv_memc.o(i.app_MEMC_IRQn_Handler)
    i.app_MIPI_RX_IRQn_Handler               0x00013990   Section        0  drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler)
    i.app_MIPI_TX_IRQn_Handler               0x00013c28   Section        0  drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler)
    i.app_PWMDET_IRQn_Handler                0x00013cc8   Section        0  drv_pwm.o(i.app_PWMDET_IRQn_Handler)
    i.app_SPIM_IRQn_Handler                  0x00013d10   Section        0  drv_spi_master.o(i.app_SPIM_IRQn_Handler)
    i.app_SPIS_IRQn_Handler                  0x00013d40   Section        0  hal_spi_slave.o(i.app_SPIS_IRQn_Handler)
    i.app_SWIRE_IRQn_Handler                 0x00013f40   Section        0  drv_swire.o(i.app_SWIRE_IRQn_Handler)
    i.app_SysTick_Handler                    0x00013f60   Section        0  drv_common.o(i.app_SysTick_Handler)
    i.app_TIMER0_IRQn_Handler                0x00013f78   Section        0  drv_timer.o(i.app_TIMER0_IRQn_Handler)
    i.app_TIMER1_IRQn_Handler                0x00013f82   Section        0  drv_timer.o(i.app_TIMER1_IRQn_Handler)
    i.app_TIMER2_IRQn_Handler                0x00013f8c   Section        0  drv_timer.o(i.app_TIMER2_IRQn_Handler)
    i.app_TIMER3_IRQn_Handler                0x00013f96   Section        0  drv_timer.o(i.app_TIMER3_IRQn_Handler)
    i.app_VIDC_IRQn_Handler                  0x00013fa0   Section        0  drv_vidc.o(i.app_VIDC_IRQn_Handler)
    i.app_VPRE_IRQn_Handler                  0x00013fbc   Section        0  drv_rxbr.o(i.app_VPRE_IRQn_Handler)
    i.app_WDG_IRQn_Handler                   0x00013fd8   Section        0  drv_wdg.o(i.app_WDG_IRQn_Handler)
    i.app_dma_irq_handler                    0x00014010   Section        0  drv_dma.o(i.app_dma_irq_handler)
    i.app_fls_ctrl_Handler                   0x00014020   Section        0  norflash.o(i.app_fls_ctrl_Handler)
    i.app_tp_I2C_init                        0x00014050   Section        0  app_tp_transfer.o(i.app_tp_I2C_init)
    i.app_tp_calibration_exec                0x00014074   Section        0  app_tp_st_touch.o(i.app_tp_calibration_exec)
    i.app_tp_i2cs_callback                   0x0001411c   Section        0  app_tp_transfer.o(i.app_tp_i2cs_callback)
    app_tp_i2cs_callback                     0x0001411d   Thumb Code    42  app_tp_transfer.o(i.app_tp_i2cs_callback)
    i.app_tp_init                            0x0001414c   Section        0  app_tp_transfer.o(i.app_tp_init)
    i.app_tp_m_read                          0x00014190   Section        0  app_tp_transfer.o(i.app_tp_m_read)
    i.app_tp_m_write                         0x000141b0   Section        0  app_tp_transfer.o(i.app_tp_m_write)
    i.app_tp_phone_analysis_data             0x000141b8   Section        0  app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data)
    i.app_tp_phone_clear_reset_on            0x0001450c   Section        0  app_tp_transfer.o(i.app_tp_phone_clear_reset_on)
    i.app_tp_s_read                          0x00014518   Section        0  app_tp_transfer.o(i.app_tp_s_read)
    i.app_tp_s_write                         0x00014520   Section        0  app_tp_transfer.o(i.app_tp_s_write)
    i.app_tp_screen_analysis_int             0x00014528   Section        0  app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int)
    i.app_tp_screen_init                     0x000147d4   Section        0  app_tp_transfer.o(i.app_tp_screen_init)
    i.app_tp_screen_int_callback             0x00014804   Section        0  app_tp_transfer.o(i.app_tp_screen_int_callback)
    app_tp_screen_int_callback               0x00014805   Thumb Code     8  app_tp_transfer.o(i.app_tp_screen_int_callback)
    i.app_tp_transfer_screen_const           0x00014810   Section        0  app_tp_transfer.o(i.app_tp_transfer_screen_const)
    app_tp_transfer_screen_const             0x00014811   Thumb Code    50  app_tp_transfer.o(i.app_tp_transfer_screen_const)
    i.app_tp_transfer_screen_int             0x00014850   Section        0  app_tp_transfer.o(i.app_tp_transfer_screen_int)
    i.app_tp_transfer_screen_start           0x00014988   Section        0  app_tp_transfer.o(i.app_tp_transfer_screen_start)
    i.board_Init                             0x000149a0   Section        0  board.o(i.board_Init)
    i.calc_framebuffer_setting               0x000149c4   Section        0  hal_internal_vsync.o(i.calc_framebuffer_setting)
    calc_framebuffer_setting                 0x000149c5   Thumb Code   902  hal_internal_vsync.o(i.calc_framebuffer_setting)
    i.ceil                                   0x00014d90   Section        0  ceil.o(i.ceil)
    i.check_mipi_rx_tx_video_info            0x00014e58   Section        0  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    check_mipi_rx_tx_video_info              0x00014e59   Thumb Code    44  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    i.check_pkt_buf_rev                      0x00014e84   Section        0  hal_internal_vsync.o(i.check_pkt_buf_rev)
    check_pkt_buf_rev                        0x00014e85   Thumb Code    90  hal_internal_vsync.o(i.check_pkt_buf_rev)
    i.dcs_packet_fifo_alloc                  0x00014f18   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    i.dcs_packet_fifo_init                   0x00014f70   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    i.dcs_packet_free_fifo_header            0x00014f88   Section        0  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    i.dcs_packet_get_fifo_header             0x00014fcc   Section        0  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    i.dcs_sw_filter                          0x00014ff0   Section        0  hal_internal_vsync.o(i.dcs_sw_filter)
    dcs_sw_filter                            0x00014ff1   Thumb Code    24  hal_internal_vsync.o(i.dcs_sw_filter)
    i.delayMs                                0x0001500c   Section        0  tau_delay.o(i.delayMs)
    i.delayUs                                0x00015024   Section        0  tau_delay.o(i.delayUs)
    i.drv_ap_rst_trig_edge_detect            0x00015048   Section        0  drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect)
    i.drv_chip_info_get_info                 0x00015080   Section        0  drv_chip_info.o(i.drv_chip_info_get_info)
    i.drv_chip_info_init                     0x0001508c   Section        0  drv_chip_info.o(i.drv_chip_info_init)
    i.drv_chip_rx_info_check                 0x000150cc   Section        0  drv_chip_info.o(i.drv_chip_rx_info_check)
    i.drv_chip_rx_init_done                  0x00015194   Section        0  drv_chip_info.o(i.drv_chip_rx_init_done)
    i.drv_common_enable_systick              0x000151a8   Section        0  drv_common.o(i.drv_common_enable_systick)
    i.drv_common_system_init                 0x00015200   Section        0  drv_common.o(i.drv_common_system_init)
    i.drv_crgu_config_reset_modules          0x00015208   Section        0  drv_crgu.o(i.drv_crgu_config_reset_modules)
    i.drv_crgu_set_ahb_pre_div               0x00015218   Section        0  drv_crgu.o(i.drv_crgu_set_ahb_pre_div)
    i.drv_crgu_set_ahb_src                   0x0001522c   Section        0  drv_crgu.o(i.drv_crgu_set_ahb_src)
    i.drv_crgu_set_clock                     0x00015240   Section        0  drv_crgu.o(i.drv_crgu_set_clock)
    i.drv_crgu_set_dpi_mux_src               0x00015260   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_mux_src)
    i.drv_crgu_set_dpi_pre_div               0x00015274   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_pre_div)
    i.drv_crgu_set_dpi_pre_src               0x0001528c   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_pre_src)
    i.drv_crgu_set_dsc_core_div              0x000152a0   Section        0  drv_crgu.o(i.drv_crgu_set_dsc_core_div)
    i.drv_crgu_set_dsco_src                  0x000152b4   Section        0  drv_crgu.o(i.drv_crgu_set_dsco_src)
    i.drv_crgu_set_dsco_src_div              0x000152c8   Section        0  drv_crgu.o(i.drv_crgu_set_dsco_src_div)
    i.drv_crgu_set_fb_div                    0x000152dc   Section        0  drv_crgu.o(i.drv_crgu_set_fb_div)
    i.drv_crgu_set_fb_src                    0x000152f0   Section        0  drv_crgu.o(i.drv_crgu_set_fb_src)
    i.drv_crgu_set_lcdc_div                  0x00015304   Section        0  drv_crgu.o(i.drv_crgu_set_lcdc_div)
    i.drv_crgu_set_lcdc_src                  0x00015318   Section        0  drv_crgu.o(i.drv_crgu_set_lcdc_src)
    i.drv_crgu_set_mipi_cfg_src              0x0001532c   Section        0  drv_crgu.o(i.drv_crgu_set_mipi_cfg_src)
    i.drv_crgu_set_mipi_ref_src              0x00015340   Section        0  drv_crgu.o(i.drv_crgu_set_mipi_ref_src)
    i.drv_crgu_set_reset                     0x00015358   Section        0  drv_crgu.o(i.drv_crgu_set_reset)
    i.drv_crgu_set_rxbr_div                  0x00015370   Section        0  drv_crgu.o(i.drv_crgu_set_rxbr_div)
    i.drv_crgu_set_rxbr_src                  0x00015384   Section        0  drv_crgu.o(i.drv_crgu_set_rxbr_src)
    i.drv_crgu_set_vidc_src                  0x00015398   Section        0  drv_crgu.o(i.drv_crgu_set_vidc_src)
    i.drv_dma_clear_flag                     0x000153ac   Section        0  drv_dma.o(i.drv_dma_clear_flag)
    i.drv_dma_create_handle                  0x000153c4   Section        0  drv_dma.o(i.drv_dma_create_handle)
    i.drv_dma_disenable_channel              0x000153e0   Section        0  drv_dma.o(i.drv_dma_disenable_channel)
    i.drv_dma_enable_channel                 0x000153f0   Section        0  drv_dma.o(i.drv_dma_enable_channel)
    i.drv_dma_enable_channel_interrupts      0x00015400   Section        0  drv_dma.o(i.drv_dma_enable_channel_interrupts)
    i.drv_dma_get_channel_flag               0x00015424   Section        0  drv_dma.o(i.drv_dma_get_channel_flag)
    i.drv_dma_irq_handler                    0x00015430   Section        0  drv_dma.o(i.drv_dma_irq_handler)
    i.drv_dma_prepar_transfer                0x000154c0   Section        0  drv_dma.o(i.drv_dma_prepar_transfer)
    i.drv_dma_set_burst                      0x000154d2   Section        0  drv_dma.o(i.drv_dma_set_burst)
    i.drv_dma_set_callback                   0x000154ec   Section        0  drv_dma.o(i.drv_dma_set_callback)
    i.drv_dma_set_transfer                   0x000154f4   Section        0  drv_dma.o(i.drv_dma_set_transfer)
    i.drv_dsc_dec_convert_pps_rc_parameter   0x00015538   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter)
    i.drv_dsc_dec_disable                    0x0001556e   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    i.drv_dsc_dec_enable                     0x0001557c   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    i.drv_dsc_dec_get_nslc                   0x000155f0   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    i.drv_dsc_dec_set_u8_pps                 0x000155fa   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps)
    i.drv_dsi_rx_calc_ipi_tx_delay           0x00015624   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    i.drv_dsi_rx_enable_irq                  0x00015728   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    i.drv_dsi_rx_get_color_bpp               0x00015768   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    drv_dsi_rx_get_color_bpp                 0x00015769   Thumb Code    62  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    i.drv_dsi_rx_get_color_pcc               0x000157b8   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    drv_dsi_rx_get_color_pcc                 0x000157b9   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    i.drv_dsi_rx_get_compression_en          0x000157d4   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    i.drv_dsi_rx_get_max_ret_size            0x000157dc   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size)
    i.drv_dsi_rx_power_up                    0x000157e2   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    i.drv_dsi_rx_set_ctrl_cfg                0x000157f0   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    i.drv_dsi_rx_set_ddi_cfg                 0x00015810   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    i.drv_dsi_rx_set_inten                   0x00015820   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    i.drv_dsi_rx_set_ipi_cfg                 0x00015824   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    i.drv_dsi_rx_set_lane_swap               0x00015834   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    i.drv_dsi_rx_set_resp_cnt                0x0001587a   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    i.drv_dsi_rx_set_up_phy                  0x000158a0   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    i.drv_dsi_rx_shut_down                   0x00015990   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    i.drv_dsi_tx_command_header              0x0001599e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    i.drv_dsi_tx_command_mode_cfg            0x000159b2   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    i.drv_dsi_tx_command_put_payload         0x00015a1e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    i.drv_dsi_tx_config_eotp                 0x00015a22   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    i.drv_dsi_tx_config_int                  0x00015a3a   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    i.drv_dsi_tx_dpi_lpcmd_time              0x00015a42   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    i.drv_dsi_tx_dpi_mode                    0x00015a4a   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    i.drv_dsi_tx_dpi_polarity                0x00015a54   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    i.drv_dsi_tx_edpi_cmd_size               0x00015a78   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    i.drv_dsi_tx_get_cmd_status              0x00015a7c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    i.drv_dsi_tx_mode                        0x00015a80   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    i.drv_dsi_tx_phy_clock_lane_auto_lp      0x00015a84   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    i.drv_dsi_tx_phy_clock_lane_req_hs       0x00015a9c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    i.drv_dsi_tx_phy_lane_mode               0x00015ab6   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    i.drv_dsi_tx_phy_status_ready            0x00015ac2   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    i.drv_dsi_tx_phy_status_stopstate        0x00015b26   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    i.drv_dsi_tx_phy_test_setup              0x00015b64   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    i.drv_dsi_tx_phy_time_cfg                0x00015c70   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    i.drv_dsi_tx_powerup                     0x00015c8e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    i.drv_dsi_tx_response_mode               0x00015c96   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    i.drv_dsi_tx_set_bta_ack                 0x00015cb2   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    i.drv_dsi_tx_set_esc_div                 0x00015cca   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    i.drv_dsi_tx_set_int                     0x00015cd8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    i.drv_dsi_tx_set_time_out_div            0x00015d0c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    i.drv_dsi_tx_set_video_chunk             0x00015d1c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    i.drv_dsi_tx_set_video_timing            0x00015d24   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    i.drv_dsi_tx_shutdown                    0x00015d46   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    i.drv_dsi_tx_timeout_cfg                 0x00015d4e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    i.drv_dsi_tx_video_mode_cfg              0x00015d74   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    i.drv_dsi_tx_video_mode_disable_hact_cmd 0x00015e1e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_disable_hact_cmd)
    i.drv_dsi_tx_video_mode_set_lp_cmd       0x00015e34   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd)
    i.drv_efuse_enter_inactive               0x00015e4c   Section        0  drv_efuse.o(i.drv_efuse_enter_inactive)
    i.drv_efuse_int_enable                   0x00015e6c   Section        0  drv_efuse.o(i.drv_efuse_int_enable)
    i.drv_efuse_read                         0x00015e78   Section        0  drv_efuse.o(i.drv_efuse_read)
    i.drv_efuse_read_req                     0x00015eaa   Section        0  drv_efuse.o(i.drv_efuse_read_req)
    i.drv_gpio_get_input_data                0x00015ec4   Section        0  drv_gpio.o(i.drv_gpio_get_input_data)
    i.drv_gpio_register_ap_reset_callback    0x00015edc   Section        0  drv_gpio.o(i.drv_gpio_register_ap_reset_callback)
    i.drv_gpio_register_callback             0x00015ee8   Section        0  drv_gpio.o(i.drv_gpio_register_callback)
    i.drv_gpio_set_int                       0x00015efc   Section        0  drv_gpio.o(i.drv_gpio_set_int)
    i.drv_gpio_set_ioe                       0x00015f40   Section        0  drv_gpio.o(i.drv_gpio_set_ioe)
    i.drv_gpio_set_mode0                     0x00015f60   Section        0  drv_gpio.o(i.drv_gpio_set_mode0)
    i.drv_gpio_set_mode1                     0x00015f70   Section        0  drv_gpio.o(i.drv_gpio_set_mode1)
    i.drv_gpio_set_mode2                     0x00015f80   Section        0  drv_gpio.o(i.drv_gpio_set_mode2)
    i.drv_gpio_set_mode3                     0x00015f90   Section        0  drv_gpio.o(i.drv_gpio_set_mode3)
    i.drv_gpio_set_output_data               0x00015fa0   Section        0  hal_gpio.o(i.drv_gpio_set_output_data)
    drv_gpio_set_output_data                 0x00015fa1   Thumb Code    26  hal_gpio.o(i.drv_gpio_set_output_data)
    i.drv_gpio_set_pull_state                0x00015fc0   Section        0  drv_gpio.o(i.drv_gpio_set_pull_state)
    i.drv_i2c_dma_callback                   0x000160f0   Section        0  drv_i2c_dma.o(i.drv_i2c_dma_callback)
    drv_i2c_dma_callback                     0x000160f1   Thumb Code    40  drv_i2c_dma.o(i.drv_i2c_dma_callback)
    i.drv_i2c_dma_init                       0x00016124   Section        0  drv_i2c_dma.o(i.drv_i2c_dma_init)
    i.drv_i2c_enable_rx_dma                  0x000161d0   Section        0  drv_i2c_dma.o(i.drv_i2c_enable_rx_dma)
    i.drv_i2c_enable_tx_dma                  0x000161ea   Section        0  drv_i2c_dma.o(i.drv_i2c_enable_tx_dma)
    i.drv_i2c_m_clear_it_pending_bit         0x00016204   Section        0  drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit)
    i.drv_i2c_m_enable                       0x00016264   Section        0  drv_i2c_master.o(i.drv_i2c_m_enable)
    i.drv_i2c_m_enable_intr                  0x00016274   Section        0  drv_i2c_master.o(i.drv_i2c_m_enable_intr)
    i.drv_i2c_m_set_callback                 0x000162ac   Section        0  drv_i2c_master.o(i.drv_i2c_m_set_callback)
    i.drv_i2c_master_init                    0x000162b8   Section        0  drv_i2c_master.o(i.drv_i2c_master_init)
    i.drv_i2c_master_read_dma                0x00016344   Section        0  drv_i2c_dma.o(i.drv_i2c_master_read_dma)
    i.drv_i2c_master_write_dma               0x000163a0   Section        0  drv_i2c_dma.o(i.drv_i2c_master_write_dma)
    i.drv_i2c_master_write_read_cmd          0x000163dc   Section        0  drv_i2c_dma.o(i.drv_i2c_master_write_read_cmd)
    drv_i2c_master_write_read_cmd            0x000163dd   Thumb Code    46  drv_i2c_dma.o(i.drv_i2c_master_write_read_cmd)
    i.drv_i2c_s_clear_it_pending_bit         0x0001640c   Section        0  drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit)
    i.drv_i2c_s_enable_intr                  0x00016468   Section        0  drv_i2c_slave.o(i.drv_i2c_s_enable_intr)
    i.drv_i2c_s_get_fifo_status              0x0001649c   Section        0  drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status)
    i.drv_i2c_s_set_callback                 0x000164b8   Section        0  drv_i2c_slave.o(i.drv_i2c_s_set_callback)
    i.drv_i2c_s_write_data                   0x000164c4   Section        0  drv_i2c_slave.o(i.drv_i2c_s_write_data)
    i.drv_i2c_set_dma_irq_callback           0x000164e4   Section        0  drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback)
    i.drv_i2c_slave_init                     0x0001653c   Section        0  drv_i2c_slave.o(i.drv_i2c_slave_init)
    i.drv_i2c_slave_write_dma                0x00016580   Section        0  drv_i2c_dma.o(i.drv_i2c_slave_write_dma)
    i.drv_lcdc_config_bypass                 0x0001659c   Section        0  drv_lcdc.o(i.drv_lcdc_config_bypass)
    i.drv_lcdc_config_ccm                    0x000165b4   Section        0  drv_lcdc.o(i.drv_lcdc_config_ccm)
    i.drv_lcdc_config_disp_mode              0x000165e4   Section        0  drv_lcdc.o(i.drv_lcdc_config_disp_mode)
    i.drv_lcdc_config_dpi_polarity           0x000165fa   Section        0  drv_lcdc.o(i.drv_lcdc_config_dpi_polarity)
    i.drv_lcdc_config_dpi_timing             0x0001661e   Section        0  drv_lcdc.o(i.drv_lcdc_config_dpi_timing)
    i.drv_lcdc_config_edpi_mode              0x00016644   Section        0  drv_lcdc.o(i.drv_lcdc_config_edpi_mode)
    i.drv_lcdc_config_endianness             0x0001665a   Section        0  drv_lcdc.o(i.drv_lcdc_config_endianness)
    i.drv_lcdc_config_input_size             0x00016670   Section        0  drv_lcdc.o(i.drv_lcdc_config_input_size)
    i.drv_lcdc_config_int                    0x0001667c   Section        0  drv_lcdc.o(i.drv_lcdc_config_int)
    i.drv_lcdc_config_int_single             0x0001669a   Section        0  drv_lcdc.o(i.drv_lcdc_config_int_single)
    i.drv_lcdc_config_overwrite              0x000166bc   Section        0  drv_lcdc.o(i.drv_lcdc_config_overwrite)
    i.drv_lcdc_config_overwrite_rgb          0x000166de   Section        0  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    i.drv_lcdc_config_partial_display_area   0x000166ea   Section        0  drv_lcdc.o(i.drv_lcdc_config_partial_display_area)
    i.drv_lcdc_config_partial_display_enable 0x00016704   Section        0  drv_lcdc.o(i.drv_lcdc_config_partial_display_enable)
    i.drv_lcdc_config_scale_up_coef          0x00016726   Section        0  drv_lcdc.o(i.drv_lcdc_config_scale_up_coef)
    i.drv_lcdc_config_scale_up_step          0x00016740   Section        0  drv_lcdc.o(i.drv_lcdc_config_scale_up_step)
    i.drv_lcdc_config_src_parameter          0x0001674c   Section        0  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    i.drv_lcdc_config_thresh                 0x00016798   Section        0  drv_lcdc.o(i.drv_lcdc_config_thresh)
    i.drv_lcdc_ctrl_flow                     0x0001679e   Section        0  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    i.drv_lcdc_enable_shadow_reg             0x000167b0   Section        0  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    i.drv_lcdc_set_int                       0x000167d0   Section        0  drv_lcdc.o(i.drv_lcdc_set_int)
    i.drv_lcdc_set_video_hw_mode             0x00016804   Section        0  drv_lcdc.o(i.drv_lcdc_set_video_hw_mode)
    i.drv_lcdc_start                         0x00016818   Section        0  drv_lcdc.o(i.drv_lcdc_start)
    i.drv_memc_clear_status                  0x00016838   Section        0  drv_memc.o(i.drv_memc_clear_status)
    i.drv_memc_enable_irq                    0x00016844   Section        0  drv_memc.o(i.drv_memc_enable_irq)
    i.drv_memc_gen_a_tear_signal             0x00016884   Section        0  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    i.drv_memc_get_status                    0x00016890   Section        0  drv_memc.o(i.drv_memc_get_status)
    i.drv_memc_rate_transfer_sel             0x000168a2   Section        0  drv_memc.o(i.drv_memc_rate_transfer_sel)
    i.drv_memc_sel_vsync                     0x000168b2   Section        0  drv_memc.o(i.drv_memc_sel_vsync)
    i.drv_memc_set_active_height             0x000168c0   Section        0  drv_memc.o(i.drv_memc_set_active_height)
    i.drv_memc_set_data_mode                 0x000168d4   Section        0  drv_memc.o(i.drv_memc_set_data_mode)
    i.drv_memc_set_double_buffer             0x000168e0   Section        0  drv_memc.o(i.drv_memc_set_double_buffer)
    i.drv_memc_set_double_buffer_reverse     0x000168f0   Section        0  drv_memc.o(i.drv_memc_set_double_buffer_reverse)
    i.drv_memc_set_fs_en_conditions          0x00016902   Section        0  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    i.drv_memc_set_inten                     0x00016912   Section        0  drv_memc.o(i.drv_memc_set_inten)
    i.drv_memc_set_lcdc_st_conditions        0x00016928   Section        0  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    i.drv_memc_set_ltpo_mode                 0x00016940   Section        0  drv_memc.o(i.drv_memc_set_ltpo_mode)
    i.drv_memc_set_tear_mode                 0x0001695a   Section        0  drv_memc.o(i.drv_memc_set_tear_mode)
    i.drv_memc_set_tear_waveform             0x00016968   Section        0  drv_memc.o(i.drv_memc_set_tear_waveform)
    i.drv_memc_set_vidc_sync_cnt             0x00016990   Section        0  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    i.drv_param_init_get_ccm                 0x000169a0   Section        0  drv_param_init.o(i.drv_param_init_get_ccm)
    i.drv_param_init_get_scld_filter_h       0x000169a8   Section        0  drv_param_init.o(i.drv_param_init_get_scld_filter_h)
    i.drv_param_init_get_scld_filter_v       0x000169bc   Section        0  drv_param_init.o(i.drv_param_init_get_scld_filter_v)
    i.drv_param_init_get_sclu_filter         0x000169d0   Section        0  drv_param_init.o(i.drv_param_init_get_sclu_filter)
    i.drv_param_init_set_ccm                 0x000169d8   Section        0  drv_param_init.o(i.drv_param_init_set_ccm)
    i.drv_param_init_set_scld_filter         0x000169ec   Section        0  drv_param_init.o(i.drv_param_init_set_scld_filter)
    i.drv_param_p2r_filter_init              0x00016a50   Section        0  drv_param_init.o(i.drv_param_p2r_filter_init)
    i.drv_phy_enable_calibration             0x00016a74   Section        0  drv_phy_common.o(i.drv_phy_enable_calibration)
    i.drv_phy_get_calibration                0x00016a84   Section        0  drv_phy_common.o(i.drv_phy_get_calibration)
    i.drv_phy_get_pll_para                   0x00016ac0   Section        0  drv_phy_common.o(i.drv_phy_get_pll_para)
    i.drv_phy_get_rate_para                  0x00016b20   Section        0  drv_phy_common.o(i.drv_phy_get_rate_para)
    i.drv_phy_test_clear                     0x00016b74   Section        0  drv_phy_common.o(i.drv_phy_test_clear)
    i.drv_phy_test_lock                      0x00016b84   Section        0  drv_phy_common.o(i.drv_phy_test_lock)
    i.drv_phy_test_write_1_byte              0x00016b9c   Section        0  drv_phy_common.o(i.drv_phy_test_write_1_byte)
    i.drv_phy_test_write_2_byte              0x00016bbc   Section        0  drv_phy_common.o(i.drv_phy_test_write_2_byte)
    i.drv_phy_test_write_code                0x00016be2   Section        0  drv_phy_common.o(i.drv_phy_test_write_code)
    i.drv_phy_test_write_data                0x00016c00   Section        0  drv_phy_common.o(i.drv_phy_test_write_data)
    drv_phy_test_write_data                  0x00016c01   Thumb Code    32  drv_phy_common.o(i.drv_phy_test_write_data)
    i.drv_pwr_set_cp_mode                    0x00016c20   Section        0  drv_pwr.o(i.drv_pwr_set_cp_mode)
    i.drv_pwr_set_pvd_mode                   0x00016c40   Section        0  drv_pwr.o(i.drv_pwr_set_pvd_mode)
    i.drv_pwr_set_system_clk_src             0x00016c58   Section        0  drv_pwr.o(i.drv_pwr_set_system_clk_src)
    i.drv_rx_phy_test_clear                  0x00016c88   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_clear)
    drv_rx_phy_test_clear                    0x00016c89   Thumb Code    12  drv_dsi_rx.o(i.drv_rx_phy_test_clear)
    i.drv_rx_phy_test_lock                   0x00016c94   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_lock)
    drv_rx_phy_test_lock                     0x00016c95   Thumb Code    16  drv_dsi_rx.o(i.drv_rx_phy_test_lock)
    i.drv_rx_phy_test_write_1_byte           0x00016ca4   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte)
    drv_rx_phy_test_write_1_byte             0x00016ca5   Thumb Code    20  drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte)
    i.drv_rx_phy_test_write_2_byte           0x00016cb8   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte)
    drv_rx_phy_test_write_2_byte             0x00016cb9   Thumb Code    22  drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte)
    i.drv_rxbr_clear_pkt_buffer              0x00016cce   Section        0  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    i.drv_rxbr_clear_status0                 0x00016cd8   Section        0  drv_rxbr.o(i.drv_rxbr_clear_status0)
    i.drv_rxbr_enable_irq                    0x00016cdc   Section        0  drv_rxbr.o(i.drv_rxbr_enable_irq)
    i.drv_rxbr_frame_drop_cfg                0x00016d38   Section        0  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    i.drv_rxbr_get_clk                       0x00016d4c   Section        0  drv_rxbr.o(i.drv_rxbr_get_clk)
    i.drv_rxbr_get_col_addr                  0x00016d88   Section        0  drv_rxbr.o(i.drv_rxbr_get_col_addr)
    i.drv_rxbr_get_int_source                0x00016d8c   Section        0  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    drv_rxbr_get_int_source                  0x00016d8d   Thumb Code    18  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    i.drv_rxbr_get_page_addr                 0x00016d9e   Section        0  drv_rxbr.o(i.drv_rxbr_get_page_addr)
    i.drv_rxbr_get_status0                   0x00016da2   Section        0  hal_internal_vsync.o(i.drv_rxbr_get_status0)
    drv_rxbr_get_status0                     0x00016da3   Thumb Code    18  hal_internal_vsync.o(i.drv_rxbr_get_status0)
    i.drv_rxbr_hline_rcv0_cfg                0x00016db4   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg)
    i.drv_rxbr_hline_rcv_cfg                 0x00016dc0   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    i.drv_rxbr_register_irq0_callback        0x00016dc8   Section        0  drv_rxbr.o(i.drv_rxbr_register_irq0_callback)
    i.drv_rxbr_register_irq1_callback        0x00016dd4   Section        0  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    i.drv_rxbr_set_ack_pkt_header            0x00016de0   Section        0  drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header)
    i.drv_rxbr_set_cmd_filter                0x00016df4   Section        0  drv_rxbr.o(i.drv_rxbr_set_cmd_filter)
    i.drv_rxbr_set_color_format              0x00016ec0   Section        0  drv_rxbr.o(i.drv_rxbr_set_color_format)
    i.drv_rxbr_set_inten                     0x00016ed4   Section        0  drv_rxbr.o(i.drv_rxbr_set_inten)
    i.drv_rxbr_set_ltpo_drop_th              0x00016ee8   Section        0  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    i.drv_rxbr_set_usr_cfg                   0x00016ef8   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    i.drv_rxbr_set_usr_col                   0x00016f1e   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    i.drv_rxbr_set_usr_row                   0x00016f26   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    i.drv_spi_m_read_data                    0x00016f30   Section        0  drv_spi_master.o(i.drv_spi_m_read_data)
    i.drv_swire_set_int                      0x00016f50   Section        0  drv_swire.o(i.drv_swire_set_int)
    i.drv_sys_cfg_clear_all_int              0x00016f98   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    i.drv_sys_cfg_clear_pending              0x00016fa4   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    i.drv_sys_cfg_sel_ap_rst_lvl_trig        0x00016fcc   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig)
    i.drv_sys_cfg_sel_ap_rst_trig            0x00016fe4   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig)
    i.drv_sys_cfg_sel_gpio_group             0x00017000   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group)
    i.drv_sys_cfg_sel_int_trig               0x00017024   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig)
    i.drv_sys_cfg_set_dma_rx_req             0x00017048   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req)
    i.drv_sys_cfg_set_dma_tx_req             0x00017058   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req)
    i.drv_sys_cfg_set_int                    0x00017068   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    i.drv_timer_clear_status_flags           0x0001708c   Section        0  drv_timer.o(i.drv_timer_clear_status_flags)
    i.drv_timer_enable                       0x000170a6   Section        0  drv_timer.o(i.drv_timer_enable)
    i.drv_timer_get_instance                 0x000170c8   Section        0  drv_timer.o(i.drv_timer_get_instance)
    i.drv_timer_get_prescaler                0x000170d8   Section        0  drv_timer.o(i.drv_timer_get_prescaler)
    i.drv_timer_handle_interrupt             0x000170e8   Section        0  drv_timer.o(i.drv_timer_handle_interrupt)
    drv_timer_handle_interrupt               0x000170e9   Thumb Code    62  drv_timer.o(i.drv_timer_handle_interrupt)
    i.drv_timer_register_callback            0x0001712c   Section        0  drv_timer.o(i.drv_timer_register_callback)
    i.drv_timer_set_current_count            0x00017140   Section        0  drv_timer.o(i.drv_timer_set_current_count)
    i.drv_timer_set_int                      0x0001714c   Section        0  drv_timer.o(i.drv_timer_set_int)
    i.drv_timer_set_match                    0x00017194   Section        0  drv_timer.o(i.drv_timer_set_match)
    i.drv_timer_set_prescaler                0x000171a0   Section        0  drv_timer.o(i.drv_timer_set_prescaler)
    i.drv_tx_phy_test_clear                  0x000171b6   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_clear)
    drv_tx_phy_test_clear                    0x000171b7   Thumb Code    10  drv_dsi_tx.o(i.drv_tx_phy_test_clear)
    i.drv_tx_phy_test_enter                  0x000171c0   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    i.drv_tx_phy_test_exit                   0x000171dc   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    i.drv_tx_phy_test_write_1_byte           0x000171f8   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte)
    drv_tx_phy_test_write_1_byte             0x000171f9   Thumb Code    18  drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte)
    i.drv_tx_phy_test_write_2_byte           0x0001720a   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte)
    drv_tx_phy_test_write_2_byte             0x0001720b   Thumb Code    20  drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte)
    i.drv_tx_phy_test_write_code             0x0001721e   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    drv_tx_phy_test_write_code               0x0001721f   Thumb Code    16  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    i.drv_vidc_clear_irq                     0x0001722e   Section        0  drv_vidc.o(i.drv_vidc_clear_irq)
    i.drv_vidc_enable                        0x00017236   Section        0  drv_vidc.o(i.drv_vidc_enable)
    i.drv_vidc_enable_irq                    0x00017250   Section        0  drv_vidc.o(i.drv_vidc_enable_irq)
    i.drv_vidc_get_irq_status                0x00017290   Section        0  drv_vidc.o(i.drv_vidc_get_irq_status)
    i.drv_vidc_init_module_enable            0x000172a4   Section        0  drv_vidc.o(i.drv_vidc_init_module_enable)
    i.drv_vidc_register_callback             0x000172cc   Section        0  drv_vidc.o(i.drv_vidc_register_callback)
    i.drv_vidc_reset                         0x000172d8   Section        0  drv_vidc.o(i.drv_vidc_reset)
    i.drv_vidc_set_dst_parameter             0x000172de   Section        0  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    i.drv_vidc_set_irqen                     0x0001731a   Section        0  drv_vidc.o(i.drv_vidc_set_irqen)
    i.drv_vidc_set_mirror                    0x0001732e   Section        0  drv_vidc.o(i.drv_vidc_set_mirror)
    i.drv_vidc_set_p2r_hcoef0                0x0001733e   Section        0  drv_vidc.o(i.drv_vidc_set_p2r_hcoef0)
    i.drv_vidc_set_p2r_hinitb                0x00017346   Section        0  drv_vidc.o(i.drv_vidc_set_p2r_hinitb)
    i.drv_vidc_set_p2r_hinitr                0x0001736c   Section        0  drv_vidc.o(i.drv_vidc_set_p2r_hinitr)
    i.drv_vidc_set_pentile_swap              0x00017394   Section        0  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    i.drv_vidc_set_pu_ctrl                   0x000173ac   Section        0  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    i.drv_vidc_set_rotation                  0x000173b6   Section        0  drv_vidc.o(i.drv_vidc_set_rotation)
    i.drv_vidc_set_scld_hcoef0               0x000173c6   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    i.drv_vidc_set_scld_hcoef1               0x000173d0   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    i.drv_vidc_set_scld_step                 0x000173da   Section        0  drv_vidc.o(i.drv_vidc_set_scld_step)
    i.drv_vidc_set_scld_vcoef0               0x000173ec   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    i.drv_vidc_set_scld_vcoef1               0x000173f6   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    i.drv_vidc_set_src_parameter             0x00017400   Section        0  drv_vidc.o(i.drv_vidc_set_src_parameter)
    i.drv_wdg_clear_counter                  0x00017418   Section        0  drv_wdg.o(i.drv_wdg_clear_counter)
    i.drv_wdg_clear_edge_flag                0x00017428   Section        0  drv_wdg.o(i.drv_wdg_clear_edge_flag)
    drv_wdg_clear_edge_flag                  0x00017429   Thumb Code    12  drv_wdg.o(i.drv_wdg_clear_edge_flag)
    i.drv_wdg_read_edge_flag                 0x00017438   Section        0  drv_wdg.o(i.drv_wdg_read_edge_flag)
    drv_wdg_read_edge_flag                   0x00017439   Thumb Code    10  drv_wdg.o(i.drv_wdg_read_edge_flag)
    i.drv_wdg_set_int                        0x00017448   Section        0  drv_wdg.o(i.drv_wdg_set_int)
    i.fls_clr_interrupt_flag                 0x0001747c   Section        0  drv_fls.o(i.fls_clr_interrupt_flag)
    i.fputc                                  0x00017486   Section        0  tau_log.o(i.fputc)
    i.hal_dsi_rx_ctrl_create_handle          0x0001749c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    i.hal_dsi_rx_ctrl_deinit                 0x000174cc   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit)
    i.hal_dsi_rx_ctrl_dsc_async_handler      0x00017568   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler)
    i.hal_dsi_rx_ctrl_gen_a_tear_signal      0x000175ec   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal)
    i.hal_dsi_rx_ctrl_get_max_ret_size       0x00017614   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size)
    i.hal_dsi_rx_ctrl_init                   0x0001763c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    i.hal_dsi_rx_ctrl_init_clk               0x000176d4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    hal_dsi_rx_ctrl_init_clk                 0x000176d5   Thumb Code   232  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    i.hal_dsi_rx_ctrl_init_dsi_rx            0x00017804   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    hal_dsi_rx_ctrl_init_dsi_rx              0x00017805   Thumb Code   180  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    i.hal_dsi_rx_ctrl_init_memc              0x000178d8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    hal_dsi_rx_ctrl_init_memc                0x000178d9   Thumb Code   308  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    i.hal_dsi_rx_ctrl_init_rxbr              0x00017a14   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    hal_dsi_rx_ctrl_init_rxbr                0x00017a15   Thumb Code   288  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    i.hal_dsi_rx_ctrl_init_vidc              0x00017b44   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    hal_dsi_rx_ctrl_init_vidc                0x00017b45   Thumb Code   544  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    i.hal_dsi_rx_ctrl_pre_init_pps           0x00017d70   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    i.hal_dsi_rx_ctrl_send_ack_cmd           0x00017dac   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd)
    i.hal_dsi_rx_ctrl_set_cus_esc_clk        0x00017e9c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk)
    i.hal_dsi_rx_ctrl_set_cus_scld_filter    0x00017ec8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter)
    i.hal_dsi_rx_ctrl_set_cus_sync_line      0x00017f34   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line)
    i.hal_dsi_rx_ctrl_set_ipi_cfg            0x00017f68   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    hal_dsi_rx_ctrl_set_ipi_cfg              0x00017f69   Thumb Code    50  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    i.hal_dsi_rx_ctrl_set_rxbr_clk           0x00017fa0   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk)
    hal_dsi_rx_ctrl_set_rxbr_clk             0x00017fa1   Thumb Code   114  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk)
    i.hal_dsi_rx_ctrl_set_sw_tear_mode       0x00018014   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode)
    i.hal_dsi_rx_ctrl_set_tear_mode_ex       0x00018048   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex)
    i.hal_dsi_rx_ctrl_start                  0x00018058   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    i.hal_dsi_rx_ctrl_stop                   0x00018094   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop)
    i.hal_dsi_rx_ctrl_toggle_resolution      0x000180d0   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    i.hal_dsi_tx_calc_video_chunks           0x000180f0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks)
    hal_dsi_tx_calc_video_chunks             0x000180f1   Thumb Code   384  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks)
    i.hal_dsi_tx_config_params_for_lane_rate 0x00018280   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate)
    hal_dsi_tx_config_params_for_lane_rate   0x00018281   Thumb Code    42  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate)
    i.hal_dsi_tx_count_lane_rate             0x000182b4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate)
    hal_dsi_tx_count_lane_rate               0x000182b5   Thumb Code  1160  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate)
    i.hal_dsi_tx_ctrl_create_handle          0x00018784   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    i.hal_dsi_tx_ctrl_deinit                 0x000187b0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit)
    i.hal_dsi_tx_ctrl_enter_init_panel_mode  0x000187f8   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode)
    i.hal_dsi_tx_ctrl_exit_init_panel_mode   0x00018844   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode)
    i.hal_dsi_tx_ctrl_init                   0x0001886c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    i.hal_dsi_tx_ctrl_init_clk               0x00018930   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    hal_dsi_tx_ctrl_init_clk                 0x00018931   Thumb Code    36  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    i.hal_dsi_tx_ctrl_panel_reset_pin        0x00018954   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin)
    i.hal_dsi_tx_ctrl_set_ccm                0x00018960   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm)
    i.hal_dsi_tx_ctrl_set_overwrite_rgb      0x00018980   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    i.hal_dsi_tx_ctrl_set_partial_disp       0x00018994   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp)
    i.hal_dsi_tx_ctrl_set_partial_disp_area  0x000189a4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area)
    i.hal_dsi_tx_ctrl_start                  0x000189c8   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    i.hal_dsi_tx_ctrl_stop                   0x00018a34   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop)
    i.hal_dsi_tx_ctrl_write_array_cmd        0x00018a78   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd)
    i.hal_dsi_tx_ctrl_write_cmd              0x00018b50   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    i.hal_dsi_tx_init_data_mode              0x00018c00   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode)
    hal_dsi_tx_init_data_mode                0x00018c01   Thumb Code    58  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode)
    i.hal_dsi_tx_init_dpi_cfg                0x00018c44   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg)
    hal_dsi_tx_init_dpi_cfg                  0x00018c45   Thumb Code    42  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg)
    i.hal_dsi_tx_init_interrupt              0x00018c74   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt)
    hal_dsi_tx_init_interrupt                0x00018c75   Thumb Code    28  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt)
    i.hal_dsi_tx_init_phy_cfg                0x00018c94   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    hal_dsi_tx_init_phy_cfg                  0x00018c95   Thumb Code    28  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    i.hal_dsi_tx_init_remains                0x00018cb4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains)
    hal_dsi_tx_init_remains                  0x00018cb5   Thumb Code   142  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains)
    i.hal_dsi_tx_init_video_mode             0x00018d48   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode)
    hal_dsi_tx_init_video_mode               0x00018d49   Thumb Code    82  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode)
    i.hal_dsi_tx_send_cmd                    0x00018da0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    hal_dsi_tx_send_cmd                      0x00018da1   Thumb Code    60  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    i.hal_gpio_ctrl_eint                     0x00018de4   Section        0  hal_gpio.o(i.hal_gpio_ctrl_eint)
    i.hal_gpio_get_input_data                0x00018dfc   Section        0  hal_gpio.o(i.hal_gpio_get_input_data)
    i.hal_gpio_init_eint                     0x00018e10   Section        0  hal_gpio.o(i.hal_gpio_init_eint)
    i.hal_gpio_init_input                    0x00018e50   Section        0  hal_gpio.o(i.hal_gpio_init_input)
    i.hal_gpio_init_output                   0x00018e70   Section        0  hal_gpio.o(i.hal_gpio_init_output)
    i.hal_gpio_reg_eint_cb                   0x00018e98   Section        0  hal_gpio.o(i.hal_gpio_reg_eint_cb)
    i.hal_gpio_set_ap_reset_int              0x00018eb0   Section        0  hal_gpio.o(i.hal_gpio_set_ap_reset_int)
    i.hal_gpio_set_mode                      0x00018f00   Section        0  hal_gpio.o(i.hal_gpio_set_mode)
    i.hal_gpio_set_output_data               0x00018f60   Section        0  hal_gpio.o(i.hal_gpio_set_output_data)
    i.hal_gpio_set_pull_state                0x00018f68   Section        0  hal_gpio.o(i.hal_gpio_set_pull_state)
    i.hal_i2c_m_dma_init                     0x00018f88   Section        0  hal_i2c_master.o(i.hal_i2c_m_dma_init)
    i.hal_i2c_m_dma_read                     0x00018ff4   Section        0  hal_i2c_master.o(i.hal_i2c_m_dma_read)
    i.hal_i2c_m_dma_write                    0x00019014   Section        0  hal_i2c_master.o(i.hal_i2c_m_dma_write)
    i.hal_i2c_m_transfer_complate            0x00019030   Section        0  hal_i2c_master.o(i.hal_i2c_m_transfer_complate)
    i.hal_i2c_master_irq_callback            0x0001903c   Section        0  hal_i2c_master.o(i.hal_i2c_master_irq_callback)
    hal_i2c_master_irq_callback              0x0001903d   Thumb Code    24  hal_i2c_master.o(i.hal_i2c_master_irq_callback)
    i.hal_i2c_s_dma_user_callback            0x0001905c   Section        0  hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback)
    hal_i2c_s_dma_user_callback              0x0001905d   Thumb Code    12  hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback)
    i.hal_i2c_s_dma_write                    0x0001906c   Section        0  hal_i2c_slave.o(i.hal_i2c_s_dma_write)
    i.hal_i2c_s_init                         0x000190a4   Section        0  hal_i2c_slave.o(i.hal_i2c_s_init)
    i.hal_i2c_s_nonblocking_read             0x00019110   Section        0  hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read)
    i.hal_i2c_s_set_transfer                 0x00019124   Section        0  hal_i2c_slave.o(i.hal_i2c_s_set_transfer)
    i.hal_i2c_slave_irq_callback             0x00019130   Section        0  hal_i2c_slave.o(i.hal_i2c_slave_irq_callback)
    hal_i2c_slave_irq_callback               0x00019131   Thumb Code   304  hal_i2c_slave.o(i.hal_i2c_slave_irq_callback)
    i.hal_internal_init_memc                 0x0001927c   Section        0  hal_internal_vsync.o(i.hal_internal_init_memc)
    i.hal_internal_sync_get_fb_setting       0x00019360   Section        0  hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting)
    i.hal_internal_sync_input_resolution_change 0x00019370   Section        0  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    i.hal_internal_vsync_deinit              0x00019584   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    i.hal_internal_vsync_get_rx_state        0x000195a0   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state)
    i.hal_internal_vsync_get_sync_line       0x000195ac   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    i.hal_internal_vsync_get_tx_state        0x000195c4   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    i.hal_internal_vsync_init_rx             0x000195d0   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    i.hal_internal_vsync_init_tx             0x000196cc   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    i.hal_internal_vsync_set_auto_hw_filter  0x0001977c   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter)
    i.hal_internal_vsync_set_rx_state        0x00019898   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    i.hal_internal_vsync_set_sync_line       0x000198ac   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line)
    i.hal_internal_vsync_set_tear_mode       0x000198c8   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    i.hal_internal_vsync_set_tx_state        0x00019910   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    i.hal_lcdc_config_ccm                    0x00019950   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm)
    hal_lcdc_config_ccm                      0x00019951   Thumb Code    30  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm)
    i.hal_lcdc_config_remains                0x00019974   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains)
    hal_lcdc_config_remains                  0x00019975   Thumb Code    68  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains)
    i.hal_lcdc_config_rgb_to_pentile         0x000199bc   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile)
    hal_lcdc_config_rgb_to_pentile           0x000199bd   Thumb Code    14  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile)
    i.hal_lcdc_config_upscaler               0x000199d0   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler)
    hal_lcdc_config_upscaler                 0x000199d1   Thumb Code   348  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler)
    i.hal_lcdc_init_cfg                      0x00019b34   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    hal_lcdc_init_cfg                        0x00019b35   Thumb Code    60  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    i.hal_lcdc_init_clk                      0x00019b74   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    hal_lcdc_init_clk                        0x00019b75   Thumb Code   376  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    i.hal_lcdc_init_interrupt                0x00019cf4   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt)
    hal_lcdc_init_interrupt                  0x00019cf5   Thumb Code    58  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt)
    i.hal_spi_m_clear_rxfifo                 0x00019d34   Section        0  hal_spi_master.o(i.hal_spi_m_clear_rxfifo)
    i.hal_system_enable_systick              0x00019d42   Section        0  hal_system.o(i.hal_system_enable_systick)
    i.hal_system_init                        0x00019d4c   Section        0  hal_system.o(i.hal_system_init)
    i.hal_system_init_console                0x00019dd4   Section        0  hal_system.o(i.hal_system_init_console)
    i.hal_system_set_phy_calibration         0x00019df0   Section        0  hal_system.o(i.hal_system_set_phy_calibration)
    i.hal_system_set_pvd                     0x00019df8   Section        0  hal_system.o(i.hal_system_set_pvd)
    i.hal_system_set_vcc                     0x00019e00   Section        0  hal_system.o(i.hal_system_set_vcc)
    i.hal_timer_init                         0x00019e08   Section        0  hal_timer.o(i.hal_timer_init)
    i.hal_timer_start                        0x00019e24   Section        0  hal_timer.o(i.hal_timer_start)
    i.hal_uart_init                          0x00019e74   Section        0  hal_uart.o(i.hal_uart_init)
    i.hal_uart_transmit_blocking             0x00019f00   Section        0  hal_uart.o(i.hal_uart_transmit_blocking)
    i.handle_init                            0x00019f10   Section        0  irq_redirect .o(i.handle_init)
    i.init_mipi_tx                           0x0001a020   Section        0  ap_demo.o(i.init_mipi_tx)
    init_mipi_tx                             0x0001a021   Thumb Code   104  ap_demo.o(i.init_mipi_tx)
    i.init_panel                             0x0001a090   Section        0  ap_demo.o(i.init_panel)
    init_panel                               0x0001a091   Thumb Code   142  ap_demo.o(i.init_panel)
    i.main                                   0x0001a128   Section        0  main.o(i.main)
    i.open_mipi_rx                           0x0001a134   Section        0  ap_demo.o(i.open_mipi_rx)
    open_mipi_rx                             0x0001a135   Thumb Code   162  ap_demo.o(i.open_mipi_rx)
    i.pps_update_handle                      0x0001a1fc   Section        0  ap_demo.o(i.pps_update_handle)
    pps_update_handle                        0x0001a1fd   Thumb Code    90  ap_demo.o(i.pps_update_handle)
    i.rx_get_dcs_packet_data                 0x0001a2bc   Section        0  hal_internal_vsync.o(i.rx_get_dcs_packet_data)
    rx_get_dcs_packet_data                   0x0001a2bd   Thumb Code   654  hal_internal_vsync.o(i.rx_get_dcs_packet_data)
    i.rx_partial_update                      0x0001a6b0   Section        0  hal_internal_vsync.o(i.rx_partial_update)
    rx_partial_update                        0x0001a6b1   Thumb Code   304  hal_internal_vsync.o(i.rx_partial_update)
    i.rx_receive_packet                      0x0001a7f0   Section        0  hal_internal_vsync.o(i.rx_receive_packet)
    rx_receive_packet                        0x0001a7f1   Thumb Code   128  hal_internal_vsync.o(i.rx_receive_packet)
    i.rx_receive_pps                         0x0001a87c   Section        0  hal_internal_vsync.o(i.rx_receive_pps)
    rx_receive_pps                           0x0001a87d   Thumb Code   268  hal_internal_vsync.o(i.rx_receive_pps)
    i.rxbr_irq0_callback                     0x0001a9fc   Section        0  hal_internal_vsync.o(i.rxbr_irq0_callback)
    rxbr_irq0_callback                       0x0001a9fd   Thumb Code   158  hal_internal_vsync.o(i.rxbr_irq0_callback)
    i.rxbr_irq1_callback                     0x0001aaa0   Section        0  hal_internal_vsync.o(i.rxbr_irq1_callback)
    rxbr_irq1_callback                       0x0001aaa1   Thumb Code   222  hal_internal_vsync.o(i.rxbr_irq1_callback)
    i.soft_gen_te                            0x0001ac10   Section        0  hal_internal_vsync.o(i.soft_gen_te)
    soft_gen_te                              0x0001ac11   Thumb Code   116  hal_internal_vsync.o(i.soft_gen_te)
    i.soft_timer3_cb                         0x0001ac9c   Section        0  ap_demo.o(i.soft_timer3_cb)
    soft_timer3_cb                           0x0001ac9d   Thumb Code    36  ap_demo.o(i.soft_timer3_cb)
    i.sqrt                                   0x0001accc   Section        0  sqrt.o(i.sqrt)
    i.tp_heartbeat_exec                      0x0001ad14   Section        0  ap_demo.o(i.tp_heartbeat_exec)
    i.vidc_callback                          0x0001ad7c   Section        0  hal_internal_vsync.o(i.vidc_callback)
    vidc_callback                            0x0001ad7d   Thumb Code   194  hal_internal_vsync.o(i.vidc_callback)
    i.vpre_err_reset                         0x0001ae64   Section        0  hal_internal_vsync.o(i.vpre_err_reset)
    vpre_err_reset                           0x0001ae65   Thumb Code   184  hal_internal_vsync.o(i.vpre_err_reset)
    i.vsync_set_te_mode                      0x0001af34   Section        0  hal_internal_vsync.o(i.vsync_set_te_mode)
    vsync_set_te_mode                        0x0001af35   Thumb Code   254  hal_internal_vsync.o(i.vsync_set_te_mode)
    .constdata                               0x0001b0d0   Section     9400  ap_demo.o(.constdata)
    g_cus_rx_dcs_execute_table               0x0001b0d0   Data         108  ap_demo.o(.constdata)
    .constdata                               0x0001d588   Section       32  app_tp_st_touch.o(.constdata)
    .constdata                               0x0001d5a8   Section      210  hal_gpio.o(.constdata)
    s_gpio_map                               0x0001d5a8   Data         120  hal_gpio.o(.constdata)
    s_gpio_perf                              0x0001d620   Data          90  hal_gpio.o(.constdata)
    .constdata                               0x0001d67a   Section     5286  app_tp_for_custom_s8.o(.constdata)
    .constdata                               0x0001eb20   Section        1  app_tp_for_custom_s8.o(.constdata)
    .constdata                               0x0001eb24   Section        8  drv_param_init.o(.constdata)
    .constdata                               0x0001eb2c   Section      390  drv_phy_common.o(.constdata)
    phy_para_mapping_h                       0x0001eb2c   Data         184  drv_phy_common.o(.constdata)
    phy_para_mapping_l                       0x0001ebe4   Data         128  drv_phy_common.o(.constdata)
    phy_data_high_map                        0x0001ec64   Data          48  drv_phy_common.o(.constdata)
    phy_data_lp_map                          0x0001ec94   Data          30  drv_phy_common.o(.constdata)
    .conststring                             0x0001ecb4   Section       72  hal_dsi_rx_ctrl.o(.conststring)
    .conststring                             0x0001ecfc   Section      308  hal_internal_vsync.o(.conststring)
    .ARM.__AT_0x00070100                     0x00070100   Section      192  irq_redirect .o(.ARM.__AT_0x00070100)
    .data                                    0x000701d0   Section      556  ap_demo.o(.data)
    start_display_on                         0x000701d0   Data           1  ap_demo.o(.data)
    g_need_enter_sleep_mode                  0x000701d1   Data           1  ap_demo.o(.data)
    g_exit_sleep_mode                        0x000701d2   Data           1  ap_demo.o(.data)
    S21_G991B_frame_update                   0x000701d3   Data           1  ap_demo.o(.data)
    panel_display_done                       0x000701d4   Data           1  ap_demo.o(.data)
    flag_0a                                  0x000701d8   Data           1  ap_demo.o(.data)
    flag_5a                                  0x000701d9   Data           1  ap_demo.o(.data)
    flag_c9_43                               0x000701da   Data           1  ap_demo.o(.data)
    ret_7f_count                             0x000701db   Data           1  ap_demo.o(.data)
    ret_a1_count                             0x000701dc   Data           1  ap_demo.o(.data)
    ret_a2_count                             0x000701dd   Data           1  ap_demo.o(.data)
    ret_c6_count                             0x000701de   Data           1  ap_demo.o(.data)
    ret_c7_count                             0x000701df   Data           1  ap_demo.o(.data)
    ret_c8_count                             0x000701e0   Data           1  ap_demo.o(.data)
    ret_c9_count                             0x000701e1   Data           1  ap_demo.o(.data)
    frame_rate                               0x000701e2   Data           1  ap_demo.o(.data)
    g_rx_ctrl_handle                         0x000701ec   Data           4  ap_demo.o(.data)
    g_tx_ctrl_handle                         0x000701f0   Data           4  ap_demo.o(.data)
    value_reg_df                             0x000701f8   Data           4  ap_demo.o(.data)
    .data                                    0x000703fc   Section       23  app_tp_transfer.o(.data)
    s_spim_write                             0x000703fc   Data           1  app_tp_transfer.o(.data)
    s_screen_int_flag                        0x000703fd   Data           1  app_tp_transfer.o(.data)
    s_phone_reset_flag                       0x000703fe   Data           1  app_tp_transfer.o(.data)
    s_screen_int_transfer_status             0x000703ff   Data           1  app_tp_transfer.o(.data)
    s_screen_const_transfer_count            0x00070401   Data           1  app_tp_transfer.o(.data)
    screen_int_transfer_count                0x00070402   Data           1  app_tp_transfer.o(.data)
    screen_int_transfer_buffer_ready         0x00070403   Data           1  app_tp_transfer.o(.data)
    .data                                    0x00070413   Section       40  app_tp_st_touch.o(.data)
    s_calibration_flag                       0x00070413   Data           1  app_tp_st_touch.o(.data)
    s_calibration_correct_flag               0x00070414   Data           1  app_tp_st_touch.o(.data)
    .data                                    0x0007043c   Section        8  hal_dsi_rx_ctrl.o(.data)
    g_hw_auto_filter                         0x0007043c   Data           1  hal_dsi_rx_ctrl.o(.data)
    g_esc_clk                                0x00070440   Data           4  hal_dsi_rx_ctrl.o(.data)
    .data                                    0x00070444   Section        1  hal_dsi_tx_ctrl.o(.data)
    g_tx_mode                                0x00070444   Data           1  hal_dsi_tx_ctrl.o(.data)
    .data                                    0x00070445   Section        1  hal_i2c_master.o(.data)
    s_i2c_m_transfer_end                     0x00070445   Data           1  hal_i2c_master.o(.data)
    .data                                    0x00070448   Section       28  hal_i2c_slave.o(.data)
    s_txbuffer_complate                      0x00070448   Data           1  hal_i2c_slave.o(.data)
    s_i2c_s_dma_end                          0x00070449   Data           1  hal_i2c_slave.o(.data)
    s_i2c_s_receive_cnt                      0x0007044a   Data           1  hal_i2c_slave.o(.data)
    s_hal_slave_rxbuffer                     0x0007044c   Data           4  hal_i2c_slave.o(.data)
    s_hal_slave_rxbuffer_size                0x00070450   Data           4  hal_i2c_slave.o(.data)
    hal_i2c_s_callback                       0x00070454   Data           4  hal_i2c_slave.o(.data)
    s_receive_count                          0x00070458   Data           4  hal_i2c_slave.o(.data)
    s_tx_buffer_t                            0x0007045c   Data           4  hal_i2c_slave.o(.data)
    tx_sum                                   0x00070460   Data           4  hal_i2c_slave.o(.data)
    .data                                    0x00070464   Section      228  app_tp_for_custom_s8.o(.data)
    app_tp_count                             0x0007046e   Data           1  app_tp_for_custom_s8.o(.data)
    phone_85_flag                            0x0007046f   Data           1  app_tp_for_custom_s8.o(.data)
    phone_F6_flag                            0x00070470   Data           1  app_tp_for_custom_s8.o(.data)
    phone_E4_flag                            0x00070471   Data           1  app_tp_for_custom_s8.o(.data)
    phone_72_flag                            0x00070472   Data           1  app_tp_for_custom_s8.o(.data)
    phone_75_flag                            0x00070473   Data           1  app_tp_for_custom_s8.o(.data)
    phone_92_flag                            0x00070474   Data           1  app_tp_for_custom_s8.o(.data)
    phone_74_flag                            0x00070475   Data           1  app_tp_for_custom_s8.o(.data)
    u16CoordY                                0x00070478   Data           2  app_tp_for_custom_s8.o(.data)
    u16CoordX                                0x0007047a   Data           2  app_tp_for_custom_s8.o(.data)
    u16CoordY_back                           0x0007047c   Data           2  app_tp_for_custom_s8.o(.data)
    u16CoordX_back                           0x0007047e   Data           2  app_tp_for_custom_s8.o(.data)
    .data                                    0x00070548   Section        1  app_tp_for_custom_s8.o(.data)
    .data                                    0x00070549   Section        1  app_tp_for_custom_s8.o(.data)
    .data                                    0x0007054a   Section        1  app_tp_for_custom_s8.o(.data)
    .data                                    0x0007054b   Section        3  app_tp_for_custom_s8.o(.data)
    .data                                    0x0007054e   Section        5  app_tp_for_custom_s8.o(.data)
    .data                                    0x00070554   Section       48  app_tp_for_custom_s8.o(.data)
    .data                                    0x00070584   Section       18  norflash.o(.data)
    tmprg                                    0x0007058c   Data           4  norflash.o(.data)
    .data                                    0x00070598   Section       12  drv_common.o(.data)
    s_my_tick                                0x00070598   Data           4  drv_common.o(.data)
    .data                                    0x000705a4   Section        4  drv_gpio.o(.data)
    g_ap_reset_cb                            0x000705a4   Data           4  drv_gpio.o(.data)
    .data                                    0x000705a8   Section        8  drv_i2c_dma.o(.data)
    i2c0_dma_callback                        0x000705a8   Data           4  drv_i2c_dma.o(.data)
    i2c1_dma_callback                        0x000705ac   Data           4  drv_i2c_dma.o(.data)
    .data                                    0x000705b0   Section        4  drv_i2c_master.o(.data)
    i2c1_intr_callback                       0x000705b0   Data           4  drv_i2c_master.o(.data)
    .data                                    0x000705b4   Section        8  drv_i2c_slave.o(.data)
    i2c0_intr_callback                       0x000705b4   Data           4  drv_i2c_slave.o(.data)
    .data                                    0x000705bc   Section     1188  drv_param_init.o(.data)
    .data                                    0x00070a60   Section        4  drv_spi_master.o(.data)
    SPIM_intr_callback                       0x00070a60   Data           4  drv_spi_master.o(.data)
    .data                                    0x00070a64   Section        1  drv_sys_cfg.o(.data)
    sg_ap_rstn_trigger_type                  0x00070a64   Data           1  drv_sys_cfg.o(.data)
    .data                                    0x00070a68   Section       80  drv_timer.o(.data)
    sg_timer_info                            0x00070a68   Data          80  drv_timer.o(.data)
    .data                                    0x00070ab8   Section        4  hal_internal_vsync.o(.data)
    sg_cur_te_info                           0x00070ab8   Data           4  hal_internal_vsync.o(.data)
    .data                                    0x00070abc   Section        8  drv_rxbr.o(.data)
    .data                                    0x00070ac4   Section        4  drv_vidc.o(.data)
    .data                                    0x00070ac8   Section        1  drv_phy_common.o(.data)
    g_phy_calibration                        0x00070ac8   Data           1  drv_phy_common.o(.data)
    .data                                    0x00070acc   Section       12  drv_chip_info.o(.data)
    sg_chip_info                             0x00070acc   Data           4  drv_chip_info.o(.data)
    sg_chip_function                         0x00070ad0   Data           4  drv_chip_info.o(.data)
    sg_chip_encrypt                          0x00070ad4   Data           4  drv_chip_info.o(.data)
    .data                                    0x00070ad8   Section       12  drv_pwm.o(.data)
    s_pwm_type                               0x00070ad8   Data           1  drv_pwm.o(.data)
    s_pwm_cb                                 0x00070adc   Data           8  drv_pwm.o(.data)
    .data                                    0x00070ae4   Section        8  drv_swire.o(.data)
    s_swire_cb                               0x00070ae4   Data           8  drv_swire.o(.data)
    .data                                    0x00070aec   Section        8  drv_uart.o(.data)
    s_UartFcrReg                             0x00070aec   Data           4  drv_uart.o(.data)
    uart_userData                            0x00070af0   Data           4  drv_uart.o(.data)
    .data                                    0x00070af4   Section       12  drv_wdg.o(.data)
    sg_wdg_repeat                            0x00070af4   Data           1  drv_wdg.o(.data)
    sg_wdg_cb                                0x00070af8   Data           8  drv_wdg.o(.data)
    .data                                    0x00070b00   Section        4  stdout.o(.data)
    .data                                    0x00070b04   Section        4  errno.o(.data)
    _errno                                   0x00070b04   Data           4  errno.o(.data)
    .bss                                     0x00070b08   Section      400  app_tp_transfer.o(.bss)
    s_screen_read_buffer                     0x00070b08   Data         200  app_tp_transfer.o(.bss)
    s_phone_read_buffer                      0x00070bd0   Data         200  app_tp_transfer.o(.bss)
    .bss                                     0x00070c98   Section       12  app_tp_st_touch.o(.bss)
    .bss                                     0x00070ca4   Section      192  hal_dsi_rx_ctrl.o(.bss)
    g_rx_ctrl_handle                         0x00070ca4   Data         192  hal_dsi_rx_ctrl.o(.bss)
    .bss                                     0x00070d64   Section       72  hal_dsi_tx_ctrl.o(.bss)
    g_tx_ctrl_handle                         0x00070d64   Data          72  hal_dsi_tx_ctrl.o(.bss)
    .bss                                     0x00070dac   Section      256  tau_log.o(.bss)
    .bss                                     0x00070eac   Section      208  hal_uart.o(.bss)
    .bss                                     0x00070f7c   Section       28  drv_dma.o(.bss)
    s_dma_handle                             0x00070f7c   Data          28  drv_dma.o(.bss)
    .bss                                     0x00070f98   Section       64  drv_gpio.o(.bss)
    s_gpio_cb                                0x00070f98   Data          64  drv_gpio.o(.bss)
    .bss                                     0x00070fd8   Section      320  drv_i2c_dma.o(.bss)
    i2c0_dma_slave_handle                    0x00070fd8   Data         160  drv_i2c_dma.o(.bss)
    i2c1_dma_master_handle                   0x00071078   Data         160  drv_i2c_dma.o(.bss)
    .bss                                     0x00071118   Section     2392  hal_internal_vsync.o(.bss)
    g_imm_buffer                             0x00071950   Data         255  hal_internal_vsync.o(.bss)
    sg_te_info                               0x00071a50   Data          12  hal_internal_vsync.o(.bss)
    g_imm_packet                             0x00071a5c   Data          20  hal_internal_vsync.o(.bss)
    .bss                                     0x00071a70   Section     4144  dcs_packet_fifo.o(.bss)
    .bss                                     0x00072aa0   Section       32  hal_spi_slave.o(.bss)
    STACK                                    0x00072ac0   Section     4096  startup_armcm0.o(STACK)

    Global Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    BuildAttributes$$THM_ISAv3M$S$PE$A:L22$X:L11$S22$IEEE1$IW$USESV6$~STKCKD$USESV7$~SHL$OTIME$ROPI$IEEEJ$EBA8$MICROLIB$REQ8$PRES8$EABIv2 0x00000000   Number         0  anon$$obj.o ABSOLUTE
    __ARM_use_no_argv                        0x00000000   Number         0  main.o ABSOLUTE
    _printf_a                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_c                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_charcount                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_d                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_e                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_f                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_flags                            0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_dec                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_hex                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_g                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_i                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_int_dec                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_l                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ll                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lld                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lli                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llo                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llu                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llx                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_dec                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_hex                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_oct                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ls                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_mbtowc                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_n                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_o                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_p                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_percent                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_pre_padding                      0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_return_value                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_s                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_sizespec                         0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_str                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_signed                  0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_unsigned                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_u                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wctomb                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_widthprec                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_x                                0x00000000   Number         0  stubs.o ABSOLUTE
    __cpp_initialize__aeabi_                  - Undefined Weak Reference
    __cxa_finalize                            - Undefined Weak Reference
    _clock_init                               - Undefined Weak Reference
    _microlib_exit                            - Undefined Weak Reference
    __Vectors_Size                           0x000000c0   Number         0  startup_armcm0.o ABSOLUTE
    __Vectors                                0x00010000   Data           4  startup_armcm0.o(RESET)
    __Vectors_End                            0x000100c0   Data           0  startup_armcm0.o(RESET)
    __main                                   0x000100c1   Thumb Code     0  entry.o(.ARM.Collect$$$$00000000)
    _main_stk                                0x000100c1   Thumb Code     0  entry2.o(.ARM.Collect$$$$00000001)
    _main_scatterload                        0x000100c5   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    __main_after_scatterload                 0x000100c9   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    _main_clock                              0x000100c9   Thumb Code     0  entry7b.o(.ARM.Collect$$$$00000008)
    _main_cpp_init                           0x000100c9   Thumb Code     0  entry8b.o(.ARM.Collect$$$$0000000A)
    _main_init                               0x000100c9   Thumb Code     0  entry9a.o(.ARM.Collect$$$$0000000B)
    __rt_final_cpp                           0x000100d1   Thumb Code     0  entry10a.o(.ARM.Collect$$$$0000000D)
    __rt_final_exit                          0x000100d1   Thumb Code     0  entry11a.o(.ARM.Collect$$$$0000000F)
    Reset_Handler                            0x000100d5   Thumb Code    28  startup_armcm0.o(.text)
    NMI_Handler                              0x000100f1   Thumb Code     2  startup_armcm0.o(.text)
    SVC_Handler                              0x000100f5   Thumb Code     2  startup_armcm0.o(.text)
    PendSV_Handler                           0x000100f7   Thumb Code     2  startup_armcm0.o(.text)
    OTP_IRQn_Handler                         0x00010123   Thumb Code     2  startup_armcm0.o(.text)
    PVD_IRQn_Handler                         0x00010127   Thumb Code     2  startup_armcm0.o(.text)
    __aeabi_uidiv                            0x0001014d   Thumb Code     0  uidiv.o(.text)
    __aeabi_uidivmod                         0x0001014d   Thumb Code    44  uidiv.o(.text)
    __aeabi_idiv                             0x00010179   Thumb Code     0  idiv.o(.text)
    __aeabi_idivmod                          0x00010179   Thumb Code    40  idiv.o(.text)
    __aeabi_memcpy                           0x000101a1   Thumb Code    36  memcpya.o(.text)
    __aeabi_memcpy4                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memcpy8                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memset                           0x000101c5   Thumb Code    14  memseta.o(.text)
    __aeabi_memset4                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memset8                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr                           0x000101d3   Thumb Code     4  memseta.o(.text)
    __aeabi_memclr4                          0x000101d3   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr8                          0x000101d3   Thumb Code     0  memseta.o(.text)
    _memset$wrapper                          0x000101d7   Thumb Code    18  memseta.o(.text)
    __aeabi_fadd                             0x000101e9   Thumb Code   162  fadd.o(.text)
    __aeabi_fsub                             0x0001028b   Thumb Code     8  fadd.o(.text)
    __aeabi_frsub                            0x00010293   Thumb Code     8  fadd.o(.text)
    __aeabi_fmul                             0x0001029b   Thumb Code   122  fmul.o(.text)
    __aeabi_fdiv                             0x00010315   Thumb Code   124  fdiv.o(.text)
    __ARM_scalbnf                            0x00010391   Thumb Code    24  fscalb.o(.text)
    scalbnf                                  0x00010391   Thumb Code     0  fscalb.o(.text)
    __aeabi_dadd                             0x000103a9   Thumb Code   328  dadd.o(.text)
    __aeabi_dsub                             0x000104f1   Thumb Code    12  dadd.o(.text)
    __aeabi_drsub                            0x000104fd   Thumb Code    12  dadd.o(.text)
    __aeabi_dmul                             0x0001050d   Thumb Code   202  dmul.o(.text)
    __aeabi_ddiv                             0x000105dd   Thumb Code   234  ddiv.o(.text)
    __aeabi_i2f                              0x000106cd   Thumb Code    22  fflti.o(.text)
    __aeabi_ui2f                             0x000106e3   Thumb Code    14  ffltui.o(.text)
    __aeabi_ui2d                             0x000106f1   Thumb Code    24  dfltui.o(.text)
    __aeabi_f2iz                             0x0001070d   Thumb Code    50  ffixi.o(.text)
    __aeabi_f2uiz                            0x0001073f   Thumb Code    40  ffixui.o(.text)
    __aeabi_d2iz                             0x00010769   Thumb Code    62  dfixi.o(.text)
    __aeabi_d2uiz                            0x000107b1   Thumb Code    50  dfixui.o(.text)
    __aeabi_f2d                              0x000107ed   Thumb Code    40  f2d.o(.text)
    __aeabi_cdcmpeq                          0x00010815   Thumb Code     0  cdcmple.o(.text)
    __aeabi_cdcmple                          0x00010815   Thumb Code    38  cdcmple.o(.text)
    __aeabi_cfrcmple                         0x0001083d   Thumb Code    20  cfrcmple.o(.text)
    __aeabi_uldivmod                         0x00010851   Thumb Code    96  uldiv.o(.text)
    __aeabi_llsl                             0x000108b1   Thumb Code    32  llshl.o(.text)
    _ll_shift_l                              0x000108b1   Thumb Code     0  llshl.o(.text)
    __aeabi_llsr                             0x000108d1   Thumb Code    34  llushr.o(.text)
    _ll_ushift_r                             0x000108d1   Thumb Code     0  llushr.o(.text)
    __aeabi_lasr                             0x000108f3   Thumb Code    38  llsshr.o(.text)
    _ll_sshift_r                             0x000108f3   Thumb Code     0  llsshr.o(.text)
    __I$use$fp                               0x00010919   Thumb Code     0  iusefp.o(.text)
    _float_round                             0x00010919   Thumb Code    16  fepilogue.o(.text)
    _float_epilogue                          0x00010929   Thumb Code   114  fepilogue.o(.text)
    _double_round                            0x0001099b   Thumb Code    26  depilogue.o(.text)
    _double_epilogue                         0x000109b5   Thumb Code   164  depilogue.o(.text)
    _dsqrt                                   0x00010a59   Thumb Code   162  dsqrt.o(.text)
    __aeabi_d2ulz                            0x00010afd   Thumb Code    54  dfixul.o(.text)
    __aeabi_cdrcmple                         0x00010b3d   Thumb Code    38  cdrcmple.o(.text)
    __scatterload                            0x00010b65   Thumb Code    28  init.o(.text)
    __scatterload_rt2                        0x00010b65   Thumb Code     0  init.o(.text)
    __decompress                             0x00010b89   Thumb Code     0  __dczerorl2.o(.text)
    __decompress1                            0x00010b89   Thumb Code    86  __dczerorl2.o(.text)
    ADC_IRQn_Handler                         0x00010be1   Thumb Code    18  irq_redirect .o(i.ADC_IRQn_Handler)
    AP_NRESET_IRQn_Handler                   0x00010bf9   Thumb Code    18  irq_redirect .o(i.AP_NRESET_IRQn_Handler)
    CRC16_2                                  0x00010c11   Thumb Code    54  app_tp_st_touch.o(i.CRC16_2)
    DMA_IRQn_Handler                         0x00010c51   Thumb Code    14  irq_redirect .o(i.DMA_IRQn_Handler)
    EXTI_INT0_IRQn_Handler                   0x00010c65   Thumb Code    22  irq_redirect .o(i.EXTI_INT0_IRQn_Handler)
    EXTI_INT1_IRQn_Handler                   0x00010c81   Thumb Code    22  irq_redirect .o(i.EXTI_INT1_IRQn_Handler)
    EXTI_INT2_IRQn_Handler                   0x00010c9d   Thumb Code    22  irq_redirect .o(i.EXTI_INT2_IRQn_Handler)
    EXTI_INT3_IRQn_Handler                   0x00010cb9   Thumb Code    22  irq_redirect .o(i.EXTI_INT3_IRQn_Handler)
    EXTI_INT4_IRQn_Handler                   0x00010cd5   Thumb Code    22  irq_redirect .o(i.EXTI_INT4_IRQn_Handler)
    EXTI_INT5_IRQn_Handler                   0x00010cf1   Thumb Code    22  irq_redirect .o(i.EXTI_INT5_IRQn_Handler)
    EXTI_INT6_IRQn_Handler                   0x00010d0d   Thumb Code    22  irq_redirect .o(i.EXTI_INT6_IRQn_Handler)
    EXTI_INT7_IRQn_Handler                   0x00010d29   Thumb Code    22  irq_redirect .o(i.EXTI_INT7_IRQn_Handler)
    FLSCTRL_IRQn_Handler                     0x00010d45   Thumb Code    14  irq_redirect .o(i.FLSCTRL_IRQn_Handler)
    Gpio_swire_output                        0x00010d59   Thumb Code    78  ap_demo.o(i.Gpio_swire_output)
    HardFault_Handler                        0x00010da9   Thumb Code    14  irq_redirect .o(i.HardFault_Handler)
    I2C0_IRQn_Handler                        0x00010dbd   Thumb Code    18  irq_redirect .o(i.I2C0_IRQn_Handler)
    I2C1_IRQn_Handler                        0x00010dd5   Thumb Code    18  irq_redirect .o(i.I2C1_IRQn_Handler)
    LCDC_IRQn_Handler                        0x00010ded   Thumb Code    18  irq_redirect .o(i.LCDC_IRQn_Handler)
    LOG_printf                               0x00010e05   Thumb Code    30  tau_log.o(i.LOG_printf)
    MEMC_IRQn_Handler                        0x00010e2d   Thumb Code    18  irq_redirect .o(i.MEMC_IRQn_Handler)
    MIPI_RX_IRQn_Handler                     0x00010e45   Thumb Code    18  irq_redirect .o(i.MIPI_RX_IRQn_Handler)
    MIPI_TX_IRQn_Handler                     0x00010e5d   Thumb Code    18  irq_redirect .o(i.MIPI_TX_IRQn_Handler)
    PWMDET_IRQn_Handler                      0x00010e75   Thumb Code    22  irq_redirect .o(i.PWMDET_IRQn_Handler)
    S20_Start_init                           0x00010e91   Thumb Code   300  app_tp_transfer.o(i.S20_Start_init)
    SPIM_IRQn_Handler                        0x00010fd5   Thumb Code    22  irq_redirect .o(i.SPIM_IRQn_Handler)
    UART_DisableDma                          0x00010ff1   Thumb Code     2  drv_uart.o(i.UART_DisableDma)
    UART_GetInstance                         0x00010ff3   Thumb Code     4  drv_uart.o(i.UART_GetInstance)
    __scatterload_null                       0x00010ff7   Thumb Code     2  handlers.o(i.__scatterload_null)
    app_UART_IRQn_Handler                    0x00010ff9   Thumb Code     8  drv_uart.o(i.app_UART_IRQn_Handler)
    s_RAM_CK                                 0x00011000   Data          20  drv_common.o(.ARM.__at_0x11000)
    SPIS_IRQn_Handler                        0x00011015   Thumb Code    22  irq_redirect .o(i.SPIS_IRQn_Handler)
    SWIRE_IRQn_Handler                       0x00011031   Thumb Code    22  irq_redirect .o(i.SWIRE_IRQn_Handler)
    SysTick_Handler                          0x0001104d   Thumb Code    18  irq_redirect .o(i.SysTick_Handler)
    TIMER0_IRQn_Handler                      0x00011065   Thumb Code    18  irq_redirect .o(i.TIMER0_IRQn_Handler)
    TIMER1_IRQn_Handler                      0x0001107d   Thumb Code    18  irq_redirect .o(i.TIMER1_IRQn_Handler)
    TIMER2_IRQn_Handler                      0x00011095   Thumb Code    18  irq_redirect .o(i.TIMER2_IRQn_Handler)
    TIMER3_IRQn_Handler                      0x000110ad   Thumb Code    18  irq_redirect .o(i.TIMER3_IRQn_Handler)
    UART0_IRQ_Handle                         0x000110c5   Thumb Code    20  drv_uart.o(i.UART0_IRQ_Handle)
    UART_IRQn_Handler                        0x000110e1   Thumb Code    18  irq_redirect .o(i.UART_IRQn_Handler)
    UART_ResetRxFIFO                         0x000110f9   Thumb Code    32  drv_uart.o(i.UART_ResetRxFIFO)
    UART_SetBaudRate                         0x0001111d   Thumb Code    72  drv_uart.o(i.UART_SetBaudRate)
    UART_SwitchSCLK                          0x00011165   Thumb Code    26  drv_uart.o(i.UART_SwitchSCLK)
    UART_TransferHandleIRQ                   0x0001117f   Thumb Code   308  drv_uart.o(i.UART_TransferHandleIRQ)
    UART_WriteBlocking                       0x000112b3   Thumb Code    26  drv_uart.o(i.UART_WriteBlocking)
    UART_init                                0x000112cd   Thumb Code   182  drv_uart.o(i.UART_init)
    VIDC_IRQn_Handler                        0x00011389   Thumb Code    18  irq_redirect .o(i.VIDC_IRQn_Handler)
    VPRE_IRQn_Handler                        0x000113a1   Thumb Code    18  irq_redirect .o(i.VPRE_IRQn_Handler)
    WDG_IRQn_Handler                         0x000113b9   Thumb Code    18  irq_redirect .o(i.WDG_IRQn_Handler)
    __0printf                                0x000113d1   Thumb Code    24  printfa.o(i.__0printf)
    __1printf                                0x000113d1   Thumb Code     0  printfa.o(i.__0printf)
    __2printf                                0x000113d1   Thumb Code     0  printfa.o(i.__0printf)
    __c89printf                              0x000113d1   Thumb Code     0  printfa.o(i.__0printf)
    printf                                   0x000113d1   Thumb Code     0  printfa.o(i.__0printf)
    __0vsprintf                              0x000113f1   Thumb Code    30  printfa.o(i.__0vsprintf)
    __1vsprintf                              0x000113f1   Thumb Code     0  printfa.o(i.__0vsprintf)
    __2vsprintf                              0x000113f1   Thumb Code     0  printfa.o(i.__0vsprintf)
    __c89vsprintf                            0x000113f1   Thumb Code     0  printfa.o(i.__0vsprintf)
    vsprintf                                 0x000113f1   Thumb Code     0  printfa.o(i.__0vsprintf)
    __ARM_clz                                0x00011415   Thumb Code    46  depilogue.o(i.__ARM_clz)
    __ARM_common_switch8                     0x00011443   Thumb Code    26  hal_dsi_rx_ctrl.o(i.__ARM_common_switch8)
    __scatterload_copy                       0x00011521   Thumb Code    14  handlers.o(i.__scatterload_copy)
    __scatterload_zeroinit                   0x0001152f   Thumb Code    14  handlers.o(i.__scatterload_zeroinit)
    __set_errno                              0x0001153d   Thumb Code     6  errno.o(i.__set_errno)
    ap_demo                                  0x00012df5   Thumb Code   284  ap_demo.o(i.ap_demo)
    ap_get_tp_calibration_status_01          0x0001301d   Thumb Code    28  app_tp_st_touch.o(i.ap_get_tp_calibration_status_01)
    ap_set_tp_calibration_04                 0x00013229   Thumb Code   138  app_tp_st_touch.o(i.ap_set_tp_calibration_04)
    ap_tp_st_touch_calibration               0x000132c1   Thumb Code   170  app_tp_st_touch.o(i.ap_tp_st_touch_calibration)
    ap_tp_st_touch_error_handler_F3          0x00013371   Thumb Code    26  app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_F3)
    ap_tp_st_touch_error_handler_FF          0x0001338b   Thumb Code    32  app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_FF)
    ap_tp_st_touch_get_calibration_success_mark 0x000133ad   Thumb Code   150  app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark)
    ap_tp_st_touch_scan_point_init           0x00013455   Thumb Code    24  app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init)
    ap_tp_st_touch_scan_point_record_event   0x00013471   Thumb Code   142  app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event)
    ap_tp_st_touch_scan_point_record_event_exec 0x00013505   Thumb Code    50  app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec)
    ap_tp_st_touch_simulate_finger_release_event 0x00013555   Thumb Code    44  app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event)
    ap_tp_st_touch_software_reset            0x00013589   Thumb Code   118  app_tp_st_touch.o(i.ap_tp_st_touch_software_reset)
    app_ADC_IRQn_Handler                     0x000136a1   Thumb Code    22  drv_rxbr.o(i.app_ADC_IRQn_Handler)
    app_AP_NRESET_IRQn_Handler               0x000136bd   Thumb Code    32  drv_gpio.o(i.app_AP_NRESET_IRQn_Handler)
    app_EXTI_INT0_IRQn_Handler               0x000136e1   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler)
    app_EXTI_INT1_IRQn_Handler               0x000136fd   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler)
    app_EXTI_INT2_IRQn_Handler               0x00013719   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler)
    app_EXTI_INT3_IRQn_Handler               0x00013735   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler)
    app_EXTI_INT4_IRQn_Handler               0x00013751   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler)
    app_EXTI_INT5_IRQn_Handler               0x0001376d   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler)
    app_EXTI_INT6_IRQn_Handler               0x00013789   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler)
    app_EXTI_INT7_IRQn_Handler               0x000137a5   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler)
    app_HardFault_Handler                    0x000137c1   Thumb Code    12  drv_common.o(i.app_HardFault_Handler)
    app_I2C0_IRQn_Handler                    0x00013809   Thumb Code     8  drv_i2c_slave.o(i.app_I2C0_IRQn_Handler)
    app_I2C1_IRQn_Handler                    0x00013819   Thumb Code     8  drv_i2c_master.o(i.app_I2C1_IRQn_Handler)
    app_LCDC_IRQn_Handler                    0x00013829   Thumb Code    98  hal_internal_vsync.o(i.app_LCDC_IRQn_Handler)
    app_MEMC_IRQn_Handler                    0x00013909   Thumb Code   132  drv_memc.o(i.app_MEMC_IRQn_Handler)
    app_MIPI_RX_IRQn_Handler                 0x00013991   Thumb Code   232  drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler)
    app_MIPI_TX_IRQn_Handler                 0x00013c29   Thumb Code    56  drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler)
    app_PWMDET_IRQn_Handler                  0x00013cc9   Thumb Code    62  drv_pwm.o(i.app_PWMDET_IRQn_Handler)
    app_SPIM_IRQn_Handler                    0x00013d11   Thumb Code    34  drv_spi_master.o(i.app_SPIM_IRQn_Handler)
    app_SPIS_IRQn_Handler                    0x00013d41   Thumb Code   500  hal_spi_slave.o(i.app_SPIS_IRQn_Handler)
    app_SWIRE_IRQn_Handler                   0x00013f41   Thumb Code    28  drv_swire.o(i.app_SWIRE_IRQn_Handler)
    app_SysTick_Handler                      0x00013f61   Thumb Code    20  drv_common.o(i.app_SysTick_Handler)
    app_TIMER0_IRQn_Handler                  0x00013f79   Thumb Code    10  drv_timer.o(i.app_TIMER0_IRQn_Handler)
    app_TIMER1_IRQn_Handler                  0x00013f83   Thumb Code    10  drv_timer.o(i.app_TIMER1_IRQn_Handler)
    app_TIMER2_IRQn_Handler                  0x00013f8d   Thumb Code    10  drv_timer.o(i.app_TIMER2_IRQn_Handler)
    app_TIMER3_IRQn_Handler                  0x00013f97   Thumb Code    10  drv_timer.o(i.app_TIMER3_IRQn_Handler)
    app_VIDC_IRQn_Handler                    0x00013fa1   Thumb Code    22  drv_vidc.o(i.app_VIDC_IRQn_Handler)
    app_VPRE_IRQn_Handler                    0x00013fbd   Thumb Code    22  drv_rxbr.o(i.app_VPRE_IRQn_Handler)
    app_WDG_IRQn_Handler                     0x00013fd9   Thumb Code    52  drv_wdg.o(i.app_WDG_IRQn_Handler)
    app_dma_irq_handler                      0x00014011   Thumb Code    10  drv_dma.o(i.app_dma_irq_handler)
    app_fls_ctrl_Handler                     0x00014021   Thumb Code    38  norflash.o(i.app_fls_ctrl_Handler)
    app_tp_I2C_init                          0x00014051   Thumb Code    26  app_tp_transfer.o(i.app_tp_I2C_init)
    app_tp_calibration_exec                  0x00014075   Thumb Code    78  app_tp_st_touch.o(i.app_tp_calibration_exec)
    app_tp_init                              0x0001414d   Thumb Code    56  app_tp_transfer.o(i.app_tp_init)
    app_tp_m_read                            0x00014191   Thumb Code    32  app_tp_transfer.o(i.app_tp_m_read)
    app_tp_m_write                           0x000141b1   Thumb Code     8  app_tp_transfer.o(i.app_tp_m_write)
    app_tp_phone_analysis_data               0x000141b9   Thumb Code   806  app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data)
    app_tp_phone_clear_reset_on              0x0001450d   Thumb Code     8  app_tp_transfer.o(i.app_tp_phone_clear_reset_on)
    app_tp_s_read                            0x00014519   Thumb Code     8  app_tp_transfer.o(i.app_tp_s_read)
    app_tp_s_write                           0x00014521   Thumb Code     8  app_tp_transfer.o(i.app_tp_s_write)
    app_tp_screen_analysis_int               0x00014529   Thumb Code   670  app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int)
    app_tp_screen_init                       0x000147d5   Thumb Code    42  app_tp_transfer.o(i.app_tp_screen_init)
    app_tp_transfer_screen_int               0x00014851   Thumb Code   250  app_tp_transfer.o(i.app_tp_transfer_screen_int)
    app_tp_transfer_screen_start             0x00014989   Thumb Code    18  app_tp_transfer.o(i.app_tp_transfer_screen_start)
    board_Init                               0x000149a1   Thumb Code    30  board.o(i.board_Init)
    ceil                                     0x00014d91   Thumb Code   180  ceil.o(i.ceil)
    dcs_packet_fifo_alloc                    0x00014f19   Thumb Code    80  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    dcs_packet_fifo_init                     0x00014f71   Thumb Code    18  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    dcs_packet_free_fifo_header              0x00014f89   Thumb Code    60  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    dcs_packet_get_fifo_header               0x00014fcd   Thumb Code    26  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    delayMs                                  0x0001500d   Thumb Code    24  tau_delay.o(i.delayMs)
    delayUs                                  0x00015025   Thumb Code    34  tau_delay.o(i.delayUs)
    drv_ap_rst_trig_edge_detect              0x00015049   Thumb Code    46  drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect)
    drv_chip_info_get_info                   0x00015081   Thumb Code     6  drv_chip_info.o(i.drv_chip_info_get_info)
    drv_chip_info_init                       0x0001508d   Thumb Code    56  drv_chip_info.o(i.drv_chip_info_init)
    drv_chip_rx_info_check                   0x000150cd   Thumb Code   122  drv_chip_info.o(i.drv_chip_rx_info_check)
    drv_chip_rx_init_done                    0x00015195   Thumb Code    16  drv_chip_info.o(i.drv_chip_rx_init_done)
    drv_common_enable_systick                0x000151a9   Thumb Code    70  drv_common.o(i.drv_common_enable_systick)
    drv_common_system_init                   0x00015201   Thumb Code     8  drv_common.o(i.drv_common_system_init)
    drv_crgu_config_reset_modules            0x00015209   Thumb Code    10  drv_crgu.o(i.drv_crgu_config_reset_modules)
    drv_crgu_set_ahb_pre_div                 0x00015219   Thumb Code    14  drv_crgu.o(i.drv_crgu_set_ahb_pre_div)
    drv_crgu_set_ahb_src                     0x0001522d   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_ahb_src)
    drv_crgu_set_clock                       0x00015241   Thumb Code    26  drv_crgu.o(i.drv_crgu_set_clock)
    drv_crgu_set_dpi_mux_src                 0x00015261   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dpi_mux_src)
    drv_crgu_set_dpi_pre_div                 0x00015275   Thumb Code    18  drv_crgu.o(i.drv_crgu_set_dpi_pre_div)
    drv_crgu_set_dpi_pre_src                 0x0001528d   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dpi_pre_src)
    drv_crgu_set_dsc_core_div                0x000152a1   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dsc_core_div)
    drv_crgu_set_dsco_src                    0x000152b5   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dsco_src)
    drv_crgu_set_dsco_src_div                0x000152c9   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dsco_src_div)
    drv_crgu_set_fb_div                      0x000152dd   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_fb_div)
    drv_crgu_set_fb_src                      0x000152f1   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_fb_src)
    drv_crgu_set_lcdc_div                    0x00015305   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_lcdc_div)
    drv_crgu_set_lcdc_src                    0x00015319   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_lcdc_src)
    drv_crgu_set_mipi_cfg_src                0x0001532d   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_mipi_cfg_src)
    drv_crgu_set_mipi_ref_src                0x00015341   Thumb Code    18  drv_crgu.o(i.drv_crgu_set_mipi_ref_src)
    drv_crgu_set_reset                       0x00015359   Thumb Code    20  drv_crgu.o(i.drv_crgu_set_reset)
    drv_crgu_set_rxbr_div                    0x00015371   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_rxbr_div)
    drv_crgu_set_rxbr_src                    0x00015385   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_rxbr_src)
    drv_crgu_set_vidc_src                    0x00015399   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_vidc_src)
    drv_dma_clear_flag                       0x000153ad   Thumb Code    24  drv_dma.o(i.drv_dma_clear_flag)
    drv_dma_create_handle                    0x000153c5   Thumb Code    22  drv_dma.o(i.drv_dma_create_handle)
    drv_dma_disenable_channel                0x000153e1   Thumb Code    16  drv_dma.o(i.drv_dma_disenable_channel)
    drv_dma_enable_channel                   0x000153f1   Thumb Code    16  drv_dma.o(i.drv_dma_enable_channel)
    drv_dma_enable_channel_interrupts        0x00015401   Thumb Code    32  drv_dma.o(i.drv_dma_enable_channel_interrupts)
    drv_dma_get_channel_flag                 0x00015425   Thumb Code    12  drv_dma.o(i.drv_dma_get_channel_flag)
    drv_dma_irq_handler                      0x00015431   Thumb Code   138  drv_dma.o(i.drv_dma_irq_handler)
    drv_dma_prepar_transfer                  0x000154c1   Thumb Code    18  drv_dma.o(i.drv_dma_prepar_transfer)
    drv_dma_set_burst                        0x000154d3   Thumb Code    26  drv_dma.o(i.drv_dma_set_burst)
    drv_dma_set_callback                     0x000154ed   Thumb Code     6  drv_dma.o(i.drv_dma_set_callback)
    drv_dma_set_transfer                     0x000154f5   Thumb Code    62  drv_dma.o(i.drv_dma_set_transfer)
    drv_dsc_dec_convert_pps_rc_parameter     0x00015539   Thumb Code    54  drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter)
    drv_dsc_dec_disable                      0x0001556f   Thumb Code    12  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    drv_dsc_dec_enable                       0x0001557d   Thumb Code    88  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    drv_dsc_dec_get_nslc                     0x000155f1   Thumb Code    10  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    drv_dsc_dec_set_u8_pps                   0x000155fb   Thumb Code    40  drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps)
    drv_dsi_rx_calc_ipi_tx_delay             0x00015625   Thumb Code   244  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    drv_dsi_rx_enable_irq                    0x00015729   Thumb Code    58  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    drv_dsi_rx_get_compression_en            0x000157d5   Thumb Code     8  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    drv_dsi_rx_get_max_ret_size              0x000157dd   Thumb Code     6  drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size)
    drv_dsi_rx_power_up                      0x000157e3   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    drv_dsi_rx_set_ctrl_cfg                  0x000157f1   Thumb Code    32  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    drv_dsi_rx_set_ddi_cfg                   0x00015811   Thumb Code    16  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    drv_dsi_rx_set_inten                     0x00015821   Thumb Code     4  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    drv_dsi_rx_set_ipi_cfg                   0x00015825   Thumb Code    16  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    drv_dsi_rx_set_lane_swap                 0x00015835   Thumb Code    70  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    drv_dsi_rx_set_resp_cnt                  0x0001587b   Thumb Code    38  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    drv_dsi_rx_set_up_phy                    0x000158a1   Thumb Code   236  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    drv_dsi_rx_shut_down                     0x00015991   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    drv_dsi_tx_command_header                0x0001599f   Thumb Code    20  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    drv_dsi_tx_command_mode_cfg              0x000159b3   Thumb Code   108  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    drv_dsi_tx_command_put_payload           0x00015a1f   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    drv_dsi_tx_config_eotp                   0x00015a23   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    drv_dsi_tx_config_int                    0x00015a3b   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    drv_dsi_tx_dpi_lpcmd_time                0x00015a43   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    drv_dsi_tx_dpi_mode                      0x00015a4b   Thumb Code    10  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    drv_dsi_tx_dpi_polarity                  0x00015a55   Thumb Code    36  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    drv_dsi_tx_edpi_cmd_size                 0x00015a79   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    drv_dsi_tx_get_cmd_status                0x00015a7d   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    drv_dsi_tx_mode                          0x00015a81   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    drv_dsi_tx_phy_clock_lane_auto_lp        0x00015a85   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    drv_dsi_tx_phy_clock_lane_req_hs         0x00015a9d   Thumb Code    26  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    drv_dsi_tx_phy_lane_mode                 0x00015ab7   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    drv_dsi_tx_phy_status_ready              0x00015ac3   Thumb Code   100  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    drv_dsi_tx_phy_status_stopstate          0x00015b27   Thumb Code    62  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    drv_dsi_tx_phy_test_setup                0x00015b65   Thumb Code   268  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    drv_dsi_tx_phy_time_cfg                  0x00015c71   Thumb Code    30  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    drv_dsi_tx_powerup                       0x00015c8f   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    drv_dsi_tx_response_mode                 0x00015c97   Thumb Code    28  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    drv_dsi_tx_set_bta_ack                   0x00015cb3   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    drv_dsi_tx_set_esc_div                   0x00015ccb   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    drv_dsi_tx_set_int                       0x00015cd9   Thumb Code    46  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    drv_dsi_tx_set_time_out_div              0x00015d0d   Thumb Code    16  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    drv_dsi_tx_set_video_chunk               0x00015d1d   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    drv_dsi_tx_set_video_timing              0x00015d25   Thumb Code    34  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    drv_dsi_tx_shutdown                      0x00015d47   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    drv_dsi_tx_timeout_cfg                   0x00015d4f   Thumb Code    38  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    drv_dsi_tx_video_mode_cfg                0x00015d75   Thumb Code   170  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    drv_dsi_tx_video_mode_disable_hact_cmd   0x00015e1f   Thumb Code    22  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_disable_hact_cmd)
    drv_dsi_tx_video_mode_set_lp_cmd         0x00015e35   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd)
    drv_efuse_enter_inactive                 0x00015e4d   Thumb Code    32  drv_efuse.o(i.drv_efuse_enter_inactive)
    drv_efuse_int_enable                     0x00015e6d   Thumb Code    12  drv_efuse.o(i.drv_efuse_int_enable)
    drv_efuse_read                           0x00015e79   Thumb Code    50  drv_efuse.o(i.drv_efuse_read)
    drv_efuse_read_req                       0x00015eab   Thumb Code    24  drv_efuse.o(i.drv_efuse_read_req)
    drv_gpio_get_input_data                  0x00015ec5   Thumb Code    20  drv_gpio.o(i.drv_gpio_get_input_data)
    drv_gpio_register_ap_reset_callback      0x00015edd   Thumb Code     6  drv_gpio.o(i.drv_gpio_register_ap_reset_callback)
    drv_gpio_register_callback               0x00015ee9   Thumb Code    14  drv_gpio.o(i.drv_gpio_register_callback)
    drv_gpio_set_int                         0x00015efd   Thumb Code    62  drv_gpio.o(i.drv_gpio_set_int)
    drv_gpio_set_ioe                         0x00015f41   Thumb Code    26  drv_gpio.o(i.drv_gpio_set_ioe)
    drv_gpio_set_mode0                       0x00015f61   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode0)
    drv_gpio_set_mode1                       0x00015f71   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode1)
    drv_gpio_set_mode2                       0x00015f81   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode2)
    drv_gpio_set_mode3                       0x00015f91   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode3)
    drv_gpio_set_pull_state                  0x00015fc1   Thumb Code   298  drv_gpio.o(i.drv_gpio_set_pull_state)
    drv_i2c_dma_init                         0x00016125   Thumb Code   146  drv_i2c_dma.o(i.drv_i2c_dma_init)
    drv_i2c_enable_rx_dma                    0x000161d1   Thumb Code    26  drv_i2c_dma.o(i.drv_i2c_enable_rx_dma)
    drv_i2c_enable_tx_dma                    0x000161eb   Thumb Code    24  drv_i2c_dma.o(i.drv_i2c_enable_tx_dma)
    drv_i2c_m_clear_it_pending_bit           0x00016205   Thumb Code    86  drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit)
    drv_i2c_m_enable                         0x00016265   Thumb Code    10  drv_i2c_master.o(i.drv_i2c_m_enable)
    drv_i2c_m_enable_intr                    0x00016275   Thumb Code    42  drv_i2c_master.o(i.drv_i2c_m_enable_intr)
    drv_i2c_m_set_callback                   0x000162ad   Thumb Code     6  drv_i2c_master.o(i.drv_i2c_m_set_callback)
    drv_i2c_master_init                      0x000162b9   Thumb Code   118  drv_i2c_master.o(i.drv_i2c_master_init)
    drv_i2c_master_read_dma                  0x00016345   Thumb Code    82  drv_i2c_dma.o(i.drv_i2c_master_read_dma)
    drv_i2c_master_write_dma                 0x000163a1   Thumb Code    50  drv_i2c_dma.o(i.drv_i2c_master_write_dma)
    drv_i2c_s_clear_it_pending_bit           0x0001640d   Thumb Code    84  drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit)
    drv_i2c_s_enable_intr                    0x00016469   Thumb Code    40  drv_i2c_slave.o(i.drv_i2c_s_enable_intr)
    drv_i2c_s_get_fifo_status                0x0001649d   Thumb Code    22  drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status)
    drv_i2c_s_set_callback                   0x000164b9   Thumb Code     6  drv_i2c_slave.o(i.drv_i2c_s_set_callback)
    drv_i2c_s_write_data                     0x000164c5   Thumb Code    26  drv_i2c_slave.o(i.drv_i2c_s_write_data)
    drv_i2c_set_dma_irq_callback             0x000164e5   Thumb Code    68  drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback)
    drv_i2c_slave_init                       0x0001653d   Thumb Code    60  drv_i2c_slave.o(i.drv_i2c_slave_init)
    drv_i2c_slave_write_dma                  0x00016581   Thumb Code    18  drv_i2c_dma.o(i.drv_i2c_slave_write_dma)
    drv_lcdc_config_bypass                   0x0001659d   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_config_bypass)
    drv_lcdc_config_ccm                      0x000165b5   Thumb Code    48  drv_lcdc.o(i.drv_lcdc_config_ccm)
    drv_lcdc_config_disp_mode                0x000165e5   Thumb Code    22  drv_lcdc.o(i.drv_lcdc_config_disp_mode)
    drv_lcdc_config_dpi_polarity             0x000165fb   Thumb Code    36  drv_lcdc.o(i.drv_lcdc_config_dpi_polarity)
    drv_lcdc_config_dpi_timing               0x0001661f   Thumb Code    38  drv_lcdc.o(i.drv_lcdc_config_dpi_timing)
    drv_lcdc_config_edpi_mode                0x00016645   Thumb Code    22  drv_lcdc.o(i.drv_lcdc_config_edpi_mode)
    drv_lcdc_config_endianness               0x0001665b   Thumb Code    22  drv_lcdc.o(i.drv_lcdc_config_endianness)
    drv_lcdc_config_input_size               0x00016671   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_config_input_size)
    drv_lcdc_config_int                      0x0001667d   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_config_int)
    drv_lcdc_config_int_single               0x0001669b   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_int_single)
    drv_lcdc_config_overwrite                0x000166bd   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_overwrite)
    drv_lcdc_config_overwrite_rgb            0x000166df   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    drv_lcdc_config_partial_display_area     0x000166eb   Thumb Code    26  drv_lcdc.o(i.drv_lcdc_config_partial_display_area)
    drv_lcdc_config_partial_display_enable   0x00016705   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_partial_display_enable)
    drv_lcdc_config_scale_up_coef            0x00016727   Thumb Code    26  drv_lcdc.o(i.drv_lcdc_config_scale_up_coef)
    drv_lcdc_config_scale_up_step            0x00016741   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_config_scale_up_step)
    drv_lcdc_config_src_parameter            0x0001674d   Thumb Code    76  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    drv_lcdc_config_thresh                   0x00016799   Thumb Code     6  drv_lcdc.o(i.drv_lcdc_config_thresh)
    drv_lcdc_ctrl_flow                       0x0001679f   Thumb Code    18  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    drv_lcdc_enable_shadow_reg               0x000167b1   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    drv_lcdc_set_int                         0x000167d1   Thumb Code    46  drv_lcdc.o(i.drv_lcdc_set_int)
    drv_lcdc_set_video_hw_mode               0x00016805   Thumb Code    20  drv_lcdc.o(i.drv_lcdc_set_video_hw_mode)
    drv_lcdc_start                           0x00016819   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_start)
    drv_memc_clear_status                    0x00016839   Thumb Code    12  drv_memc.o(i.drv_memc_clear_status)
    drv_memc_enable_irq                      0x00016845   Thumb Code    58  drv_memc.o(i.drv_memc_enable_irq)
    drv_memc_gen_a_tear_signal               0x00016885   Thumb Code    12  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    drv_memc_get_status                      0x00016891   Thumb Code    18  drv_memc.o(i.drv_memc_get_status)
    drv_memc_rate_transfer_sel               0x000168a3   Thumb Code    16  drv_memc.o(i.drv_memc_rate_transfer_sel)
    drv_memc_sel_vsync                       0x000168b3   Thumb Code    14  drv_memc.o(i.drv_memc_sel_vsync)
    drv_memc_set_active_height               0x000168c1   Thumb Code    14  drv_memc.o(i.drv_memc_set_active_height)
    drv_memc_set_data_mode                   0x000168d5   Thumb Code    12  drv_memc.o(i.drv_memc_set_data_mode)
    drv_memc_set_double_buffer               0x000168e1   Thumb Code    16  drv_memc.o(i.drv_memc_set_double_buffer)
    drv_memc_set_double_buffer_reverse       0x000168f1   Thumb Code    18  drv_memc.o(i.drv_memc_set_double_buffer_reverse)
    drv_memc_set_fs_en_conditions            0x00016903   Thumb Code    16  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    drv_memc_set_inten                       0x00016913   Thumb Code    20  drv_memc.o(i.drv_memc_set_inten)
    drv_memc_set_lcdc_st_conditions          0x00016929   Thumb Code    18  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    drv_memc_set_ltpo_mode                   0x00016941   Thumb Code    26  drv_memc.o(i.drv_memc_set_ltpo_mode)
    drv_memc_set_tear_mode                   0x0001695b   Thumb Code    14  drv_memc.o(i.drv_memc_set_tear_mode)
    drv_memc_set_tear_waveform               0x00016969   Thumb Code    34  drv_memc.o(i.drv_memc_set_tear_waveform)
    drv_memc_set_vidc_sync_cnt               0x00016991   Thumb Code    14  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    drv_param_init_get_ccm                   0x000169a1   Thumb Code     4  drv_param_init.o(i.drv_param_init_get_ccm)
    drv_param_init_get_scld_filter_h         0x000169a9   Thumb Code    12  drv_param_init.o(i.drv_param_init_get_scld_filter_h)
    drv_param_init_get_scld_filter_v         0x000169bd   Thumb Code    12  drv_param_init.o(i.drv_param_init_get_scld_filter_v)
    drv_param_init_get_sclu_filter           0x000169d1   Thumb Code     4  drv_param_init.o(i.drv_param_init_get_sclu_filter)
    drv_param_init_set_ccm                   0x000169d9   Thumb Code    14  drv_param_init.o(i.drv_param_init_set_ccm)
    drv_param_init_set_scld_filter           0x000169ed   Thumb Code    92  drv_param_init.o(i.drv_param_init_set_scld_filter)
    drv_param_p2r_filter_init                0x00016a51   Thumb Code    30  drv_param_init.o(i.drv_param_p2r_filter_init)
    drv_phy_enable_calibration               0x00016a75   Thumb Code    12  drv_phy_common.o(i.drv_phy_enable_calibration)
    drv_phy_get_calibration                  0x00016a85   Thumb Code    50  drv_phy_common.o(i.drv_phy_get_calibration)
    drv_phy_get_pll_para                     0x00016ac1   Thumb Code    88  drv_phy_common.o(i.drv_phy_get_pll_para)
    drv_phy_get_rate_para                    0x00016b21   Thumb Code    76  drv_phy_common.o(i.drv_phy_get_rate_para)
    drv_phy_test_clear                       0x00016b75   Thumb Code    16  drv_phy_common.o(i.drv_phy_test_clear)
    drv_phy_test_lock                        0x00016b85   Thumb Code    24  drv_phy_common.o(i.drv_phy_test_lock)
    drv_phy_test_write_1_byte                0x00016b9d   Thumb Code    32  drv_phy_common.o(i.drv_phy_test_write_1_byte)
    drv_phy_test_write_2_byte                0x00016bbd   Thumb Code    38  drv_phy_common.o(i.drv_phy_test_write_2_byte)
    drv_phy_test_write_code                  0x00016be3   Thumb Code    30  drv_phy_common.o(i.drv_phy_test_write_code)
    drv_pwr_set_cp_mode                      0x00016c21   Thumb Code    26  drv_pwr.o(i.drv_pwr_set_cp_mode)
    drv_pwr_set_pvd_mode                     0x00016c41   Thumb Code    18  drv_pwr.o(i.drv_pwr_set_pvd_mode)
    drv_pwr_set_system_clk_src               0x00016c59   Thumb Code    36  drv_pwr.o(i.drv_pwr_set_system_clk_src)
    drv_rxbr_clear_pkt_buffer                0x00016ccf   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    drv_rxbr_clear_status0                   0x00016cd9   Thumb Code     4  drv_rxbr.o(i.drv_rxbr_clear_status0)
    drv_rxbr_enable_irq                      0x00016cdd   Thumb Code    90  drv_rxbr.o(i.drv_rxbr_enable_irq)
    drv_rxbr_frame_drop_cfg                  0x00016d39   Thumb Code    16  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    drv_rxbr_get_clk                         0x00016d4d   Thumb Code    44  drv_rxbr.o(i.drv_rxbr_get_clk)
    drv_rxbr_get_col_addr                    0x00016d89   Thumb Code     4  drv_rxbr.o(i.drv_rxbr_get_col_addr)
    drv_rxbr_get_page_addr                   0x00016d9f   Thumb Code     4  drv_rxbr.o(i.drv_rxbr_get_page_addr)
    drv_rxbr_hline_rcv0_cfg                  0x00016db5   Thumb Code    12  drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg)
    drv_rxbr_hline_rcv_cfg                   0x00016dc1   Thumb Code     8  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    drv_rxbr_register_irq0_callback          0x00016dc9   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_register_irq0_callback)
    drv_rxbr_register_irq1_callback          0x00016dd5   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    drv_rxbr_set_ack_pkt_header              0x00016de1   Thumb Code    20  drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header)
    drv_rxbr_set_cmd_filter                  0x00016df5   Thumb Code   204  drv_rxbr.o(i.drv_rxbr_set_cmd_filter)
    drv_rxbr_set_color_format                0x00016ec1   Thumb Code    20  drv_rxbr.o(i.drv_rxbr_set_color_format)
    drv_rxbr_set_inten                       0x00016ed5   Thumb Code    20  drv_rxbr.o(i.drv_rxbr_set_inten)
    drv_rxbr_set_ltpo_drop_th                0x00016ee9   Thumb Code    16  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    drv_rxbr_set_usr_cfg                     0x00016ef9   Thumb Code    38  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    drv_rxbr_set_usr_col                     0x00016f1f   Thumb Code     8  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    drv_rxbr_set_usr_row                     0x00016f27   Thumb Code     8  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    drv_spi_m_read_data                      0x00016f31   Thumb Code    28  drv_spi_master.o(i.drv_spi_m_read_data)
    drv_swire_set_int                        0x00016f51   Thumb Code    64  drv_swire.o(i.drv_swire_set_int)
    drv_sys_cfg_clear_all_int                0x00016f99   Thumb Code     8  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    drv_sys_cfg_clear_pending                0x00016fa5   Thumb Code    32  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    drv_sys_cfg_sel_ap_rst_lvl_trig          0x00016fcd   Thumb Code    18  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig)
    drv_sys_cfg_sel_ap_rst_trig              0x00016fe5   Thumb Code    22  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig)
    drv_sys_cfg_sel_gpio_group               0x00017001   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group)
    drv_sys_cfg_sel_int_trig                 0x00017025   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig)
    drv_sys_cfg_set_dma_rx_req               0x00017049   Thumb Code    10  drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req)
    drv_sys_cfg_set_dma_tx_req               0x00017059   Thumb Code    10  drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req)
    drv_sys_cfg_set_int                      0x00017069   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    drv_timer_clear_status_flags             0x0001708d   Thumb Code    26  drv_timer.o(i.drv_timer_clear_status_flags)
    drv_timer_enable                         0x000170a7   Thumb Code    32  drv_timer.o(i.drv_timer_enable)
    drv_timer_get_instance                   0x000170c9   Thumb Code    10  drv_timer.o(i.drv_timer_get_instance)
    drv_timer_get_prescaler                  0x000170d9   Thumb Code    14  drv_timer.o(i.drv_timer_get_prescaler)
    drv_timer_register_callback              0x0001712d   Thumb Code    14  drv_timer.o(i.drv_timer_register_callback)
    drv_timer_set_current_count              0x00017141   Thumb Code    12  drv_timer.o(i.drv_timer_set_current_count)
    drv_timer_set_int                        0x0001714d   Thumb Code    68  drv_timer.o(i.drv_timer_set_int)
    drv_timer_set_match                      0x00017195   Thumb Code    12  drv_timer.o(i.drv_timer_set_match)
    drv_timer_set_prescaler                  0x000171a1   Thumb Code    22  drv_timer.o(i.drv_timer_set_prescaler)
    drv_tx_phy_test_enter                    0x000171c1   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    drv_tx_phy_test_exit                     0x000171dd   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    drv_vidc_clear_irq                       0x0001722f   Thumb Code     8  drv_vidc.o(i.drv_vidc_clear_irq)
    drv_vidc_enable                          0x00017237   Thumb Code    24  drv_vidc.o(i.drv_vidc_enable)
    drv_vidc_enable_irq                      0x00017251   Thumb Code    58  drv_vidc.o(i.drv_vidc_enable_irq)
    drv_vidc_get_irq_status                  0x00017291   Thumb Code    18  drv_vidc.o(i.drv_vidc_get_irq_status)
    drv_vidc_init_module_enable              0x000172a5   Thumb Code    36  drv_vidc.o(i.drv_vidc_init_module_enable)
    drv_vidc_register_callback               0x000172cd   Thumb Code     6  drv_vidc.o(i.drv_vidc_register_callback)
    drv_vidc_reset                           0x000172d9   Thumb Code     6  drv_vidc.o(i.drv_vidc_reset)
    drv_vidc_set_dst_parameter               0x000172df   Thumb Code    60  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    drv_vidc_set_irqen                       0x0001731b   Thumb Code    20  drv_vidc.o(i.drv_vidc_set_irqen)
    drv_vidc_set_mirror                      0x0001732f   Thumb Code    16  drv_vidc.o(i.drv_vidc_set_mirror)
    drv_vidc_set_p2r_hcoef0                  0x0001733f   Thumb Code     8  drv_vidc.o(i.drv_vidc_set_p2r_hcoef0)
    drv_vidc_set_p2r_hinitb                  0x00017347   Thumb Code    38  drv_vidc.o(i.drv_vidc_set_p2r_hinitb)
    drv_vidc_set_p2r_hinitr                  0x0001736d   Thumb Code    38  drv_vidc.o(i.drv_vidc_set_p2r_hinitr)
    drv_vidc_set_pentile_swap                0x00017395   Thumb Code    18  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    drv_vidc_set_pu_ctrl                     0x000173ad   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    drv_vidc_set_rotation                    0x000173b7   Thumb Code    16  drv_vidc.o(i.drv_vidc_set_rotation)
    drv_vidc_set_scld_hcoef0                 0x000173c7   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    drv_vidc_set_scld_hcoef1                 0x000173d1   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    drv_vidc_set_scld_step                   0x000173db   Thumb Code    18  drv_vidc.o(i.drv_vidc_set_scld_step)
    drv_vidc_set_scld_vcoef0                 0x000173ed   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    drv_vidc_set_scld_vcoef1                 0x000173f7   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    drv_vidc_set_src_parameter               0x00017401   Thumb Code    22  drv_vidc.o(i.drv_vidc_set_src_parameter)
    drv_wdg_clear_counter                    0x00017419   Thumb Code    12  drv_wdg.o(i.drv_wdg_clear_counter)
    drv_wdg_set_int                          0x00017449   Thumb Code    48  drv_wdg.o(i.drv_wdg_set_int)
    fls_clr_interrupt_flag                   0x0001747d   Thumb Code    10  drv_fls.o(i.fls_clr_interrupt_flag)
    fputc                                    0x00017487   Thumb Code    20  tau_log.o(i.fputc)
    hal_dsi_rx_ctrl_create_handle            0x0001749d   Thumb Code    42  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    hal_dsi_rx_ctrl_deinit                   0x000174cd   Thumb Code   148  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit)
    hal_dsi_rx_ctrl_dsc_async_handler        0x00017569   Thumb Code   120  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler)
    hal_dsi_rx_ctrl_gen_a_tear_signal        0x000175ed   Thumb Code    32  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal)
    hal_dsi_rx_ctrl_get_max_ret_size         0x00017615   Thumb Code    30  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size)
    hal_dsi_rx_ctrl_init                     0x0001763d   Thumb Code   144  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    hal_dsi_rx_ctrl_pre_init_pps             0x00017d71   Thumb Code    56  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    hal_dsi_rx_ctrl_send_ack_cmd             0x00017dad   Thumb Code   212  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd)
    hal_dsi_rx_ctrl_set_cus_esc_clk          0x00017e9d   Thumb Code    34  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk)
    hal_dsi_rx_ctrl_set_cus_scld_filter      0x00017ec9   Thumb Code    98  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter)
    hal_dsi_rx_ctrl_set_cus_sync_line        0x00017f35   Thumb Code    44  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line)
    hal_dsi_rx_ctrl_set_sw_tear_mode         0x00018015   Thumb Code    42  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode)
    hal_dsi_rx_ctrl_set_tear_mode_ex         0x00018049   Thumb Code    14  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex)
    hal_dsi_rx_ctrl_start                    0x00018059   Thumb Code    46  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    hal_dsi_rx_ctrl_stop                     0x00018095   Thumb Code    46  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop)
    hal_dsi_rx_ctrl_toggle_resolution        0x000180d1   Thumb Code    28  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    hal_dsi_tx_ctrl_create_handle            0x00018785   Thumb Code    34  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    hal_dsi_tx_ctrl_deinit                   0x000187b1   Thumb Code    68  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit)
    hal_dsi_tx_ctrl_enter_init_panel_mode    0x000187f9   Thumb Code    68  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode)
    hal_dsi_tx_ctrl_exit_init_panel_mode     0x00018845   Thumb Code    32  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode)
    hal_dsi_tx_ctrl_init                     0x0001886d   Thumb Code   188  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    hal_dsi_tx_ctrl_panel_reset_pin          0x00018955   Thumb Code    12  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin)
    hal_dsi_tx_ctrl_set_ccm                  0x00018961   Thumb Code    28  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm)
    hal_dsi_tx_ctrl_set_overwrite_rgb        0x00018981   Thumb Code    16  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    hal_dsi_tx_ctrl_set_partial_disp         0x00018995   Thumb Code    12  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp)
    hal_dsi_tx_ctrl_set_partial_disp_area    0x000189a5   Thumb Code    30  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area)
    hal_dsi_tx_ctrl_start                    0x000189c9   Thumb Code    94  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    hal_dsi_tx_ctrl_stop                     0x00018a35   Thumb Code    54  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop)
    hal_dsi_tx_ctrl_write_array_cmd          0x00018a79   Thumb Code   210  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd)
    hal_dsi_tx_ctrl_write_cmd                0x00018b51   Thumb Code   172  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    hal_gpio_ctrl_eint                       0x00018de5   Thumb Code    18  hal_gpio.o(i.hal_gpio_ctrl_eint)
    hal_gpio_get_input_data                  0x00018dfd   Thumb Code    18  hal_gpio.o(i.hal_gpio_get_input_data)
    hal_gpio_init_eint                       0x00018e11   Thumb Code    58  hal_gpio.o(i.hal_gpio_init_eint)
    hal_gpio_init_input                      0x00018e51   Thumb Code    28  hal_gpio.o(i.hal_gpio_init_input)
    hal_gpio_init_output                     0x00018e71   Thumb Code    34  hal_gpio.o(i.hal_gpio_init_output)
    hal_gpio_reg_eint_cb                     0x00018e99   Thumb Code    20  hal_gpio.o(i.hal_gpio_reg_eint_cb)
    hal_gpio_set_ap_reset_int                0x00018eb1   Thumb Code    76  hal_gpio.o(i.hal_gpio_set_ap_reset_int)
    hal_gpio_set_mode                        0x00018f01   Thumb Code    90  hal_gpio.o(i.hal_gpio_set_mode)
    hal_gpio_set_output_data                 0x00018f61   Thumb Code     8  hal_gpio.o(i.hal_gpio_set_output_data)
    hal_gpio_set_pull_state                  0x00018f69   Thumb Code    26  hal_gpio.o(i.hal_gpio_set_pull_state)
    hal_i2c_m_dma_init                       0x00018f89   Thumb Code    92  hal_i2c_master.o(i.hal_i2c_m_dma_init)
    hal_i2c_m_dma_read                       0x00018ff5   Thumb Code    26  hal_i2c_master.o(i.hal_i2c_m_dma_read)
    hal_i2c_m_dma_write                      0x00019015   Thumb Code    24  hal_i2c_master.o(i.hal_i2c_m_dma_write)
    hal_i2c_m_transfer_complate              0x00019031   Thumb Code     6  hal_i2c_master.o(i.hal_i2c_m_transfer_complate)
    hal_i2c_s_dma_write                      0x0001906d   Thumb Code    46  hal_i2c_slave.o(i.hal_i2c_s_dma_write)
    hal_i2c_s_init                           0x000190a5   Thumb Code    86  hal_i2c_slave.o(i.hal_i2c_s_init)
    hal_i2c_s_nonblocking_read               0x00019111   Thumb Code    14  hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read)
    hal_i2c_s_set_transfer                   0x00019125   Thumb Code     6  hal_i2c_slave.o(i.hal_i2c_s_set_transfer)
    hal_internal_init_memc                   0x0001927d   Thumb Code   146  hal_internal_vsync.o(i.hal_internal_init_memc)
    hal_internal_sync_get_fb_setting         0x00019361   Thumb Code    12  hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting)
    hal_internal_sync_input_resolution_change 0x00019371   Thumb Code   418  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    hal_internal_vsync_deinit                0x00019585   Thumb Code    24  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    hal_internal_vsync_get_rx_state          0x000195a1   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state)
    hal_internal_vsync_get_sync_line         0x000195ad   Thumb Code    18  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    hal_internal_vsync_get_tx_state          0x000195c5   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    hal_internal_vsync_init_rx               0x000195d1   Thumb Code   220  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    hal_internal_vsync_init_tx               0x000196cd   Thumb Code   172  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    hal_internal_vsync_set_auto_hw_filter    0x0001977d   Thumb Code   222  hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter)
    hal_internal_vsync_set_rx_state          0x00019899   Thumb Code    16  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    hal_internal_vsync_set_sync_line         0x000198ad   Thumb Code    22  hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line)
    hal_internal_vsync_set_tear_mode         0x000198c9   Thumb Code    64  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    hal_internal_vsync_set_tx_state          0x00019911   Thumb Code    54  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    hal_spi_m_clear_rxfifo                   0x00019d35   Thumb Code    14  hal_spi_master.o(i.hal_spi_m_clear_rxfifo)
    hal_system_enable_systick                0x00019d43   Thumb Code     8  hal_system.o(i.hal_system_enable_systick)
    hal_system_init                          0x00019d4d   Thumb Code   104  hal_system.o(i.hal_system_init)
    hal_system_init_console                  0x00019dd5   Thumb Code    28  hal_system.o(i.hal_system_init_console)
    hal_system_set_phy_calibration           0x00019df1   Thumb Code     8  hal_system.o(i.hal_system_set_phy_calibration)
    hal_system_set_pvd                       0x00019df9   Thumb Code     8  hal_system.o(i.hal_system_set_pvd)
    hal_system_set_vcc                       0x00019e01   Thumb Code     8  hal_system.o(i.hal_system_set_vcc)
    hal_timer_init                           0x00019e09   Thumb Code    26  hal_timer.o(i.hal_timer_init)
    hal_timer_start                          0x00019e25   Thumb Code    74  hal_timer.o(i.hal_timer_start)
    hal_uart_init                            0x00019e75   Thumb Code   126  hal_uart.o(i.hal_uart_init)
    hal_uart_transmit_blocking               0x00019f01   Thumb Code    12  hal_uart.o(i.hal_uart_transmit_blocking)
    handle_init                              0x00019f11   Thumb Code   140  irq_redirect .o(i.handle_init)
    main                                     0x0001a129   Thumb Code    10  main.o(i.main)
    sqrt                                     0x0001accd   Thumb Code    66  sqrt.o(i.sqrt)
    tp_heartbeat_exec                        0x0001ad15   Thumb Code    60  ap_demo.o(i.tp_heartbeat_exec)
    panel_init_code                          0x0001b13c   Data        9164  ap_demo.o(.constdata)
    wCRCTalbeAbs                             0x0001d588   Data          32  app_tp_st_touch.o(.constdata)
    phone_data_21                            0x0001d67a   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_55                            0x0001d67b   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_85_00                         0x0001d67c   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_F5_1                          0x0001d67d   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_F5_2                          0x0001d67e   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_F5_3                          0x0001d67f   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_F5_4                          0x0001d680   Data           1  app_tp_for_custom_s8.o(.constdata)
    phone_data_30                            0x0001d681   Data           2  app_tp_for_custom_s8.o(.constdata)
    phone_data_92_F0                         0x0001d683   Data           2  app_tp_for_custom_s8.o(.constdata)
    phone_data_52                            0x0001d685   Data           3  app_tp_for_custom_s8.o(.constdata)
    phone_data_92_15                         0x0001d688   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_data_A3                            0x0001d68c   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_data_A4                            0x0001d690   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_data_A5                            0x0001d694   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_data_AF                            0x0001d698   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_data_F1                            0x0001d69c   Data           4  app_tp_for_custom_s8.o(.constdata)
    phone_data_22                            0x0001d6a0   Data           5  app_tp_for_custom_s8.o(.constdata)
    phone_data_92_0A                         0x0001d6a5   Data           6  app_tp_for_custom_s8.o(.constdata)
    phone_data_F6_1                          0x0001d6ab   Data           6  app_tp_for_custom_s8.o(.constdata)
    phone_data_F6_2                          0x0001d6b1   Data           6  app_tp_for_custom_s8.o(.constdata)
    phone_data_F6_3                          0x0001d6b7   Data           6  app_tp_for_custom_s8.o(.constdata)
    phone_data_F6_4                          0x0001d6bd   Data           6  app_tp_for_custom_s8.o(.constdata)
    phone_data_60_1                          0x0001d6c3   Data          16  app_tp_for_custom_s8.o(.constdata)
    phone_data_23                            0x0001d6d3   Data          11  app_tp_for_custom_s8.o(.constdata)
    phone_data_85_02                         0x0001d6de   Data          28  app_tp_for_custom_s8.o(.constdata)
    phone_data_85_20                         0x0001d6fa   Data          28  app_tp_for_custom_s8.o(.constdata)
    phone_data_90                            0x0001d716   Data          10  app_tp_for_custom_s8.o(.constdata)
    phone_data_72_03                         0x0001d720   Data        1120  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_7401_7D01                  0x0001db80   Data         568  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_7401_7D02                  0x0001ddb8   Data         568  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_7401_7D03                  0x0001dff0   Data         568  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_7403_7D01                  0x0001e228   Data         568  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_7403_7D03                  0x0001e460   Data         568  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_7D05                       0x0001e698   Data         568  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_00                         0x0001e8d0   Data         288  app_tp_for_custom_s8.o(.constdata)
    phone_data_75_FF                         0x0001e9f0   Data         288  app_tp_for_custom_s8.o(.constdata)
    sleep_on                                 0x0001eb10   Data          16  app_tp_for_custom_s8.o(.constdata)
    screen_reg_start_data_size               0x0001eb20   Data           1  app_tp_for_custom_s8.o(.constdata)
    Region$$Table$$Base                      0x0001ee30   Number         0  anon$$obj.o(Region$$Table)
    Region$$Table$$Limit                     0x0001ee60   Number         0  anon$$obj.o(Region$$Table)
    g_fun_handle                             0x00070100   Data         192  irq_redirect .o(.ARM.__AT_0x00070100)
    phone_start_flag                         0x000701d5   Data           1  ap_demo.o(.data)
    phone_DisplayOFF_flag                    0x000701d6   Data           1  ap_demo.o(.data)
    panel_mode                               0x000701d7   Data           1  ap_demo.o(.data)
    phone_DisplayOFF_count                   0x000701e4   Data           2  ap_demo.o(.data)
    panel_r                                  0x000701e6   Data           2  ap_demo.o(.data)
    panel_g                                  0x000701e8   Data           2  ap_demo.o(.data)
    panel_b                                  0x000701ea   Data           2  ap_demo.o(.data)
    s_heartbeat                              0x000701f4   Data           4  ap_demo.o(.data)
    rx_filter_1080_h_4_96                    0x000701fc   Data         256  ap_demo.o(.data)
    rx_filter_2400_v_4_96                    0x000702fc   Data         256  ap_demo.o(.data)
    s_screen_init_complate                   0x00070400   Data           1  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data1               0x00070404   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data3               0x00070407   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data4               0x0007040a   Data           3  app_tp_transfer.o(.data)
    MI10_PRO_screen_init_data2               0x0007040d   Data           6  app_tp_transfer.o(.data)
    st_touch_init_sensor_off                 0x00070415   Data           3  app_tp_st_touch.o(.data)
    st_touch_init_sensor_on                  0x00070418   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_reset                 0x0007041b   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_FpnlInit              0x0007041e   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_PnlInit               0x00070421   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_SvCfg                 0x00070424   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_SvCx                  0x00070427   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_SvPnl                 0x0007042a   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_clearfifo             0x0007042d   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_clkreset              0x00070430   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_TuneM                 0x00070433   Data           4  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_TuneS                 0x00070437   Data           4  app_tp_st_touch.o(.data)
    phone_data_E4                            0x00070464   Data           1  app_tp_for_custom_s8.o(.data)
    tp_flag                                  0x00070465   Data           1  app_tp_for_custom_s8.o(.data)
    g_phone_output_int_pad                   0x00070466   Data           1  app_tp_for_custom_s8.o(.data)
    tp_sleep_in                              0x00070467   Data           1  app_tp_for_custom_s8.o(.data)
    tp_sleep_count                           0x00070468   Data           1  app_tp_for_custom_s8.o(.data)
    sleep_double_EN                          0x00070469   Data           1  app_tp_for_custom_s8.o(.data)
    Flag_EA_EN                               0x0007046a   Data           1  app_tp_for_custom_s8.o(.data)
    Flag_touch_count                         0x0007046b   Data           1  app_tp_for_custom_s8.o(.data)
    touchnum_bak                             0x0007046c   Data           1  app_tp_for_custom_s8.o(.data)
    Flag_blacklight_EN                       0x0007046d   Data           1  app_tp_for_custom_s8.o(.data)
    phone_data_B1                            0x00070476   Data           2  app_tp_for_custom_s8.o(.data)
    phone_reg_coord_back                     0x00070480   Data         200  app_tp_for_custom_s8.o(.data)
    g_screen_input_rst_pad                   0x00070548   Data           1  app_tp_for_custom_s8.o(.data)
    g_screen_input_int_pad                   0x00070549   Data           1  app_tp_for_custom_s8.o(.data)
    screen_data_write_1                      0x0007054a   Data           1  app_tp_for_custom_s8.o(.data)
    screen_data_write_2                      0x0007054b   Data           3  app_tp_for_custom_s8.o(.data)
    screen_data_write_3                      0x0007054e   Data           5  app_tp_for_custom_s8.o(.data)
    screen_reg_int_data                      0x00070554   Data          48  app_tp_for_custom_s8.o(.data)
    g_fls_w_cmd                              0x00070584   Data           1  norflash.o(.data)
    g_fls_r_cmd                              0x00070585   Data           1  norflash.o(.data)
    g_fls_write_en_status                    0x00070586   Data           1  norflash.o(.data)
    isFlsTransferEnd                         0x00070587   Data           1  norflash.o(.data)
    isFlsFifoReq                             0x00070588   Data           1  norflash.o(.data)
    isNandWriteCompleted                     0x00070589   Data           1  norflash.o(.data)
    isNandReadCompleted                      0x0007058a   Data           1  norflash.o(.data)
    g_fls_error_info                         0x00070590   Data           6  norflash.o(.data)
    g_systick_cb_func                        0x0007059c   Data           4  drv_common.o(.data)
    g_system_clock                           0x000705a0   Data           4  drv_common.o(.data)
    tx_byte_num                              0x000705b8   Data           4  drv_i2c_slave.o(.data)
    g_scld_fhd_filter_h                      0x000705bc   Data         256  drv_param_init.o(.data)
    g_scld_fhd_filter_v                      0x000706bc   Data         256  drv_param_init.o(.data)
    g_scld_hd_filter_h                       0x000707bc   Data         256  drv_param_init.o(.data)
    g_scld_hd_filter_v                       0x000708bc   Data         256  drv_param_init.o(.data)
    g_sclu_lanczos_filter                    0x000709bc   Data         128  drv_param_init.o(.data)
    g_ccm_setting                            0x00070a3c   Data          36  drv_param_init.o(.data)
    g_int_rxbr_irq0_cb_func                  0x00070abc   Data           4  drv_rxbr.o(.data)
    g_int_rxbr_irq1_cb_func                  0x00070ac0   Data           4  drv_rxbr.o(.data)
    g_int_vidc_cb_func                       0x00070ac4   Data           4  drv_vidc.o(.data)
    __stdout                                 0x00070b00   Data           4  stdout.o(.data)
    tp_scan_data                             0x00070c98   Data          12  app_tp_st_touch.o(.bss)
    string                                   0x00070dac   Data         256  tau_log.o(.bss)
    hal_dmahandle                            0x00070eac   Data         160  hal_uart.o(.bss)
    hal_uarthandle_dma                       0x00070f4c   Data          32  hal_uart.o(.bss)
    hal_uart_handle_global                   0x00070f6c   Data          16  hal_uart.o(.bss)
    g_vsync_hande                            0x00071118   Data          56  hal_internal_vsync.o(.bss)
    g_dcs_execute_table                      0x00071150   Data        2048  hal_internal_vsync.o(.bss)
    g_packet_fifo                            0x00071a70   Data        4144  dcs_packet_fifo.o(.bss)
    g_spis_ctrl_handle                       0x00072aa0   Data          32  hal_spi_slave.o(.bss)
    __stack_limit                            0x00072ac0   Data           0  startup_armcm0.o(STACK)
    __initial_sp                             0x00073ac0   Data           0  startup_armcm0.o(STACK)



==============================================================================

Memory Map of the image

  Image Entry point : 0x000100c1

  Load Region LR_IROM2 (Base: 0x00010000, Size: 0x0000f798, Max: 0x00010000, ABSOLUTE, COMPRESSED[0x0000f3b4])

    Execution Region ER_IROM2 (Exec base: 0x00010000, Load base: 0x00010000, Size: 0x0000ee60, Max: 0x00010000, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00010000   0x00010000   0x000000c0   Data   RO          526    RESET               startup_armcm0.o
    0x000100c0   0x000100c0   0x00000000   Code   RO         2633  * .ARM.Collect$$$$00000000  mc_p.l(entry.o)
    0x000100c0   0x000100c0   0x00000004   Code   RO         2943    .ARM.Collect$$$$00000001  mc_p.l(entry2.o)
    0x000100c4   0x000100c4   0x00000004   Code   RO         2946    .ARM.Collect$$$$00000004  mc_p.l(entry5.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         2948    .ARM.Collect$$$$00000008  mc_p.l(entry7b.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         2950    .ARM.Collect$$$$0000000A  mc_p.l(entry8b.o)
    0x000100c8   0x000100c8   0x00000008   Code   RO         2951    .ARM.Collect$$$$0000000B  mc_p.l(entry9a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         2953    .ARM.Collect$$$$0000000D  mc_p.l(entry10a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         2955    .ARM.Collect$$$$0000000F  mc_p.l(entry11a.o)
    0x000100d0   0x000100d0   0x00000004   Code   RO         2944    .ARM.Collect$$$$00002712  mc_p.l(entry2.o)
    0x000100d4   0x000100d4   0x00000078   Code   RO          527    .text               startup_armcm0.o
    0x0001014c   0x0001014c   0x0000002c   Code   RO         2636    .text               mc_p.l(uidiv.o)
    0x00010178   0x00010178   0x00000028   Code   RO         2638    .text               mc_p.l(idiv.o)
    0x000101a0   0x000101a0   0x00000024   Code   RO         2640    .text               mc_p.l(memcpya.o)
    0x000101c4   0x000101c4   0x00000024   Code   RO         2642    .text               mc_p.l(memseta.o)
    0x000101e8   0x000101e8   0x000000b2   Code   RO         2907    .text               mf_p.l(fadd.o)
    0x0001029a   0x0001029a   0x0000007a   Code   RO         2909    .text               mf_p.l(fmul.o)
    0x00010314   0x00010314   0x0000007c   Code   RO         2911    .text               mf_p.l(fdiv.o)
    0x00010390   0x00010390   0x00000018   Code   RO         2913    .text               mf_p.l(fscalb.o)
    0x000103a8   0x000103a8   0x00000164   Code   RO         2915    .text               mf_p.l(dadd.o)
    0x0001050c   0x0001050c   0x000000d0   Code   RO         2917    .text               mf_p.l(dmul.o)
    0x000105dc   0x000105dc   0x000000f0   Code   RO         2919    .text               mf_p.l(ddiv.o)
    0x000106cc   0x000106cc   0x00000016   Code   RO         2921    .text               mf_p.l(fflti.o)
    0x000106e2   0x000106e2   0x0000000e   Code   RO         2923    .text               mf_p.l(ffltui.o)
    0x000106f0   0x000106f0   0x0000001c   Code   RO         2927    .text               mf_p.l(dfltui.o)
    0x0001070c   0x0001070c   0x00000032   Code   RO         2929    .text               mf_p.l(ffixi.o)
    0x0001073e   0x0001073e   0x00000028   Code   RO         2931    .text               mf_p.l(ffixui.o)
    0x00010766   0x00010766   0x00000002   PAD
    0x00010768   0x00010768   0x00000048   Code   RO         2933    .text               mf_p.l(dfixi.o)
    0x000107b0   0x000107b0   0x0000003c   Code   RO         2935    .text               mf_p.l(dfixui.o)
    0x000107ec   0x000107ec   0x00000028   Code   RO         2937    .text               mf_p.l(f2d.o)
    0x00010814   0x00010814   0x00000028   Code   RO         2939    .text               mf_p.l(cdcmple.o)
    0x0001083c   0x0001083c   0x00000014   Code   RO         2941    .text               mf_p.l(cfrcmple.o)
    0x00010850   0x00010850   0x00000060   Code   RO         2958    .text               mc_p.l(uldiv.o)
    0x000108b0   0x000108b0   0x00000020   Code   RO         2960    .text               mc_p.l(llshl.o)
    0x000108d0   0x000108d0   0x00000022   Code   RO         2962    .text               mc_p.l(llushr.o)
    0x000108f2   0x000108f2   0x00000026   Code   RO         2964    .text               mc_p.l(llsshr.o)
    0x00010918   0x00010918   0x00000000   Code   RO         2973    .text               mc_p.l(iusefp.o)
    0x00010918   0x00010918   0x00000082   Code   RO         2974    .text               mf_p.l(fepilogue.o)
    0x0001099a   0x0001099a   0x000000be   Code   RO         2976    .text               mf_p.l(depilogue.o)
    0x00010a58   0x00010a58   0x000000a2   Code   RO         2980    .text               mf_p.l(dsqrt.o)
    0x00010afa   0x00010afa   0x00000002   PAD
    0x00010afc   0x00010afc   0x00000040   Code   RO         2982    .text               mf_p.l(dfixul.o)
    0x00010b3c   0x00010b3c   0x00000028   Code   RO         2984    .text               mf_p.l(cdrcmple.o)
    0x00010b64   0x00010b64   0x00000024   Code   RO         2986    .text               mc_p.l(init.o)
    0x00010b88   0x00010b88   0x00000056   Code   RO         2996    .text               mc_p.l(__dczerorl2.o)
    0x00010bde   0x00010bde   0x00000002   PAD
    0x00010be0   0x00010be0   0x00000018   Code   RO         2209    i.ADC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010bf8   0x00010bf8   0x00000018   Code   RO         2210    i.AP_NRESET_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c10   0x00010c10   0x00000040   Code   RO          403    i.CRC16_2           app_tp_st_touch.o
    0x00010c50   0x00010c50   0x00000014   Code   RO         2211    i.DMA_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c64   0x00010c64   0x0000001c   Code   RO         2212    i.EXTI_INT0_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c80   0x00010c80   0x0000001c   Code   RO         2213    i.EXTI_INT1_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c9c   0x00010c9c   0x0000001c   Code   RO         2214    i.EXTI_INT2_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010cb8   0x00010cb8   0x0000001c   Code   RO         2215    i.EXTI_INT3_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010cd4   0x00010cd4   0x0000001c   Code   RO         2216    i.EXTI_INT4_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010cf0   0x00010cf0   0x0000001c   Code   RO         2217    i.EXTI_INT5_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010d0c   0x00010d0c   0x0000001c   Code   RO         2218    i.EXTI_INT6_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010d28   0x00010d28   0x0000001c   Code   RO         2219    i.EXTI_INT7_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010d44   0x00010d44   0x00000014   Code   RO         2220    i.FLSCTRL_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010d58   0x00010d58   0x0000004e   Code   RO          100    i.Gpio_swire_output  ap_demo.o
    0x00010da6   0x00010da6   0x00000002   PAD
    0x00010da8   0x00010da8   0x00000014   Code   RO         2221    i.HardFault_Handler  CVWL568.lib(irq_redirect .o)
    0x00010dbc   0x00010dbc   0x00000018   Code   RO         2222    i.I2C0_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010dd4   0x00010dd4   0x00000018   Code   RO         2223    i.I2C1_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010dec   0x00010dec   0x00000018   Code   RO         2224    i.LCDC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e04   0x00010e04   0x00000028   Code   RO          890    i.LOG_printf        CVWL568.lib(tau_log.o)
    0x00010e2c   0x00010e2c   0x00000018   Code   RO         2225    i.MEMC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e44   0x00010e44   0x00000018   Code   RO         2226    i.MIPI_RX_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e5c   0x00010e5c   0x00000018   Code   RO         2227    i.MIPI_TX_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e74   0x00010e74   0x0000001c   Code   RO         2228    i.PWMDET_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e90   0x00010e90   0x00000144   Code   RO          252    i.S20_Start_init    app_tp_transfer.o
    0x00010fd4   0x00010fd4   0x0000001c   Code   RO         2229    i.SPIM_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010ff0   0x00010ff0   0x00000002   Code   RO         2493    i.UART_DisableDma   CVWL568.lib(drv_uart.o)
    0x00010ff2   0x00010ff2   0x00000004   Code   RO         2499    i.UART_GetInstance  CVWL568.lib(drv_uart.o)
    0x00010ff6   0x00010ff6   0x00000002   Code   RO         2991    i.__scatterload_null  mc_p.l(handlers.o)
    0x00010ff8   0x00010ff8   0x00000008   Code   RO         2517    i.app_UART_IRQn_Handler  CVWL568.lib(drv_uart.o)
    0x00011000   0x00011000   0x00000014   Data   RO         1142    .ARM.__at_0x11000   CVWL568.lib(drv_common.o)
    0x00011014   0x00011014   0x0000001c   Code   RO         2230    i.SPIS_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00011030   0x00011030   0x0000001c   Code   RO         2231    i.SWIRE_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x0001104c   0x0001104c   0x00000018   Code   RO         2232    i.SysTick_Handler   CVWL568.lib(irq_redirect .o)
    0x00011064   0x00011064   0x00000018   Code   RO         2233    i.TIMER0_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x0001107c   0x0001107c   0x00000018   Code   RO         2234    i.TIMER1_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00011094   0x00011094   0x00000018   Code   RO         2235    i.TIMER2_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x000110ac   0x000110ac   0x00000018   Code   RO         2236    i.TIMER3_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x000110c4   0x000110c4   0x0000001c   Code   RO         2489    i.UART0_IRQ_Handle  CVWL568.lib(drv_uart.o)
    0x000110e0   0x000110e0   0x00000018   Code   RO         2237    i.UART_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x000110f8   0x000110f8   0x00000024   Code   RO         2507    i.UART_ResetRxFIFO  CVWL568.lib(drv_uart.o)
    0x0001111c   0x0001111c   0x00000048   Code   RO         2510    i.UART_SetBaudRate  CVWL568.lib(drv_uart.o)
    0x00011164   0x00011164   0x0000001a   Code   RO         2511    i.UART_SwitchSCLK   CVWL568.lib(drv_uart.o)
    0x0001117e   0x0001117e   0x00000134   Code   RO         2513    i.UART_TransferHandleIRQ  CVWL568.lib(drv_uart.o)
    0x000112b2   0x000112b2   0x0000001a   Code   RO         2515    i.UART_WriteBlocking  CVWL568.lib(drv_uart.o)
    0x000112cc   0x000112cc   0x000000bc   Code   RO         2516    i.UART_init         CVWL568.lib(drv_uart.o)
    0x00011388   0x00011388   0x00000018   Code   RO         2238    i.VIDC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x000113a0   0x000113a0   0x00000018   Code   RO         2239    i.VPRE_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x000113b8   0x000113b8   0x00000018   Code   RO         2240    i.WDG_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x000113d0   0x000113d0   0x00000020   Code   RO         2879    i.__0printf         mc_p.l(printfa.o)
    0x000113f0   0x000113f0   0x00000024   Code   RO         2885    i.__0vsprintf       mc_p.l(printfa.o)
    0x00011414   0x00011414   0x0000002e   Code   RO         2978    i.__ARM_clz         mf_p.l(depilogue.o)
    0x00011442   0x00011442   0x0000001a   Code   RO          620    i.__ARM_common_switch8  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001145c   0x0001145c   0x00000018   Code   RO         1460    i.__NVIC_ClearPendingIRQ  CVWL568.lib(drv_i2c_master.o)
    0x00011474   0x00011474   0x00000018   Code   RO         1493    i.__NVIC_ClearPendingIRQ  CVWL568.lib(drv_i2c_slave.o)
    0x0001148c   0x0001148c   0x00000018   Code   RO         1588    i.__NVIC_ClearPendingIRQ  CVWL568.lib(drv_spi_master.o)
    0x000114a4   0x000114a4   0x00000020   Code   RO         2063    i.__NVIC_DisableIRQ  CVWL568.lib(drv_rxbr.o)
    0x000114c4   0x000114c4   0x00000018   Code   RO         2064    i.__NVIC_EnableIRQ  CVWL568.lib(drv_rxbr.o)
    0x000114dc   0x000114dc   0x00000044   Code   RO         2337    i.__NVIC_SetPriority  CVWL568.lib(hal_spi_slave.o)
    0x00011520   0x00011520   0x0000000e   Code   RO         2990    i.__scatterload_copy  mc_p.l(handlers.o)
    0x0001152e   0x0001152e   0x0000000e   Code   RO         2992    i.__scatterload_zeroinit  mc_p.l(handlers.o)
    0x0001153c   0x0001153c   0x0000000c   Code   RO         2968    i.__set_errno       mc_p.l(errno.o)
    0x00011548   0x00011548   0x00000174   Code   RO         2886    i._fp_digits        mc_p.l(printfa.o)
    0x000116bc   0x000116bc   0x000006ec   Code   RO         2887    i._printf_core      mc_p.l(printfa.o)
    0x00011da8   0x00011da8   0x00000020   Code   RO         2888    i._printf_post_padding  mc_p.l(printfa.o)
    0x00011dc8   0x00011dc8   0x0000002c   Code   RO         2889    i._printf_pre_padding  mc_p.l(printfa.o)
    0x00011df4   0x00011df4   0x0000000a   Code   RO         2891    i._sputc            mc_p.l(printfa.o)
    0x00011dfe   0x00011dfe   0x00000002   PAD
    0x00011e00   0x00011e00   0x00000ff4   Code   RO          101    i.ap_dcs_read       ap_demo.o
    0x00012df4   0x00012df4   0x0000019c   Code   RO          102    i.ap_demo           ap_demo.o
    0x00012f90   0x00012f90   0x0000008c   Code   RO          103    i.ap_get_reg_df     ap_demo.o
    0x0001301c   0x0001301c   0x00000020   Code   RO          404    i.ap_get_tp_calibration_status_01  app_tp_st_touch.o
    0x0001303c   0x0001303c   0x00000068   Code   RO          104    i.ap_reset_cb       ap_demo.o
    0x000130a4   0x000130a4   0x0000001c   Code   RO          105    i.ap_set_backlight_51  ap_demo.o
    0x000130c0   0x000130c0   0x00000044   Code   RO          106    i.ap_set_display_off  ap_demo.o
    0x00013104   0x00013104   0x00000038   Code   RO          107    i.ap_set_display_on  ap_demo.o
    0x0001313c   0x0001313c   0x0000007c   Code   RO          108    i.ap_set_enter_sleep_mode  ap_demo.o
    0x000131b8   0x000131b8   0x00000070   Code   RO          109    i.ap_set_exit_sleep_mode  ap_demo.o
    0x00013228   0x00013228   0x00000098   Code   RO          405    i.ap_set_tp_calibration_04  app_tp_st_touch.o
    0x000132c0   0x000132c0   0x000000b0   Code   RO          406    i.ap_tp_st_touch_calibration  app_tp_st_touch.o
    0x00013370   0x00013370   0x0000001a   Code   RO          407    i.ap_tp_st_touch_error_handler_F3  app_tp_st_touch.o
    0x0001338a   0x0001338a   0x00000020   Code   RO          408    i.ap_tp_st_touch_error_handler_FF  app_tp_st_touch.o
    0x000133aa   0x000133aa   0x00000002   PAD
    0x000133ac   0x000133ac   0x000000a8   Code   RO          409    i.ap_tp_st_touch_get_calibration_success_mark  app_tp_st_touch.o
    0x00013454   0x00013454   0x0000001c   Code   RO          411    i.ap_tp_st_touch_scan_point_init  app_tp_st_touch.o
    0x00013470   0x00013470   0x00000094   Code   RO          412    i.ap_tp_st_touch_scan_point_record_event  app_tp_st_touch.o
    0x00013504   0x00013504   0x00000050   Code   RO          413    i.ap_tp_st_touch_scan_point_record_event_exec  app_tp_st_touch.o
    0x00013554   0x00013554   0x00000034   Code   RO          414    i.ap_tp_st_touch_simulate_finger_release_event  app_tp_st_touch.o
    0x00013588   0x00013588   0x000000ac   Code   RO          415    i.ap_tp_st_touch_software_reset  app_tp_st_touch.o
    0x00013634   0x00013634   0x0000006c   Code   RO          110    i.ap_update_frame_rate  ap_demo.o
    0x000136a0   0x000136a0   0x0000001c   Code   RO         2065    i.app_ADC_IRQn_Handler  CVWL568.lib(drv_rxbr.o)
    0x000136bc   0x000136bc   0x00000024   Code   RO         1384    i.app_AP_NRESET_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x000136e0   0x000136e0   0x0000001c   Code   RO         1385    i.app_EXTI_INT0_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x000136fc   0x000136fc   0x0000001c   Code   RO         1386    i.app_EXTI_INT1_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00013718   0x00013718   0x0000001c   Code   RO         1387    i.app_EXTI_INT2_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00013734   0x00013734   0x0000001c   Code   RO         1388    i.app_EXTI_INT3_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00013750   0x00013750   0x0000001c   Code   RO         1389    i.app_EXTI_INT4_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x0001376c   0x0001376c   0x0000001c   Code   RO         1390    i.app_EXTI_INT5_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00013788   0x00013788   0x0000001c   Code   RO         1391    i.app_EXTI_INT6_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x000137a4   0x000137a4   0x0000001c   Code   RO         1392    i.app_EXTI_INT7_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x000137c0   0x000137c0   0x00000048   Code   RO         1134    i.app_HardFault_Handler  CVWL568.lib(drv_common.o)
    0x00013808   0x00013808   0x00000010   Code   RO         1494    i.app_I2C0_IRQn_Handler  CVWL568.lib(drv_i2c_slave.o)
    0x00013818   0x00013818   0x00000010   Code   RO         1461    i.app_I2C1_IRQn_Handler  CVWL568.lib(drv_i2c_master.o)
    0x00013828   0x00013828   0x000000e0   Code   RO         1693    i.app_LCDC_IRQn_Handler  CVWL568.lib(hal_internal_vsync.o)
    0x00013908   0x00013908   0x00000088   Code   RO         2007    i.app_MEMC_IRQn_Handler  CVWL568.lib(drv_memc.o)
    0x00013990   0x00013990   0x00000298   Code   RO         1779    i.app_MIPI_RX_IRQn_Handler  CVWL568.lib(drv_dsi_rx.o)
    0x00013c28   0x00013c28   0x000000a0   Code   RO         1835    i.app_MIPI_TX_IRQn_Handler  CVWL568.lib(drv_dsi_tx.o)
    0x00013cc8   0x00013cc8   0x00000048   Code   RO         2405    i.app_PWMDET_IRQn_Handler  CVWL568.lib(drv_pwm.o)
    0x00013d10   0x00013d10   0x00000030   Code   RO         1589    i.app_SPIM_IRQn_Handler  CVWL568.lib(drv_spi_master.o)
    0x00013d40   0x00013d40   0x00000200   Code   RO         2338    i.app_SPIS_IRQn_Handler  CVWL568.lib(hal_spi_slave.o)
    0x00013f40   0x00013f40   0x00000020   Code   RO         2470    i.app_SWIRE_IRQn_Handler  CVWL568.lib(drv_swire.o)
    0x00013f60   0x00013f60   0x00000018   Code   RO         1135    i.app_SysTick_Handler  CVWL568.lib(drv_common.o)
    0x00013f78   0x00013f78   0x0000000a   Code   RO         1652    i.app_TIMER0_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x00013f82   0x00013f82   0x0000000a   Code   RO         1653    i.app_TIMER1_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x00013f8c   0x00013f8c   0x0000000a   Code   RO         1654    i.app_TIMER2_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x00013f96   0x00013f96   0x0000000a   Code   RO         1655    i.app_TIMER3_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x00013fa0   0x00013fa0   0x0000001c   Code   RO         2130    i.app_VIDC_IRQn_Handler  CVWL568.lib(drv_vidc.o)
    0x00013fbc   0x00013fbc   0x0000001c   Code   RO         2066    i.app_VPRE_IRQn_Handler  CVWL568.lib(drv_rxbr.o)
    0x00013fd8   0x00013fd8   0x00000038   Code   RO         2576    i.app_WDG_IRQn_Handler  CVWL568.lib(drv_wdg.o)
    0x00014010   0x00014010   0x00000010   Code   RO         1246    i.app_dma_irq_handler  CVWL568.lib(drv_dma.o)
    0x00014020   0x00014020   0x00000030   Code   RO         1050    i.app_fls_ctrl_Handler  CVWL568.lib(norflash.o)
    0x00014050   0x00014050   0x00000024   Code   RO          253    i.app_tp_I2C_init   app_tp_transfer.o
    0x00014074   0x00014074   0x000000a8   Code   RO          416    i.app_tp_calibration_exec  app_tp_st_touch.o
    0x0001411c   0x0001411c   0x00000030   Code   RO          254    i.app_tp_i2cs_callback  app_tp_transfer.o
    0x0001414c   0x0001414c   0x00000044   Code   RO          255    i.app_tp_init       app_tp_transfer.o
    0x00014190   0x00014190   0x00000020   Code   RO          256    i.app_tp_m_read     app_tp_transfer.o
    0x000141b0   0x000141b0   0x00000008   Code   RO          258    i.app_tp_m_write    app_tp_transfer.o
    0x000141b8   0x000141b8   0x00000354   Code   RO          901    i.app_tp_phone_analysis_data  WL568_S21_NT37701_TP.lib(app_tp_for_custom_s8.o)
    0x0001450c   0x0001450c   0x0000000c   Code   RO          259    i.app_tp_phone_clear_reset_on  app_tp_transfer.o
    0x00014518   0x00014518   0x00000008   Code   RO          261    i.app_tp_s_read     app_tp_transfer.o
    0x00014520   0x00014520   0x00000008   Code   RO          263    i.app_tp_s_write    app_tp_transfer.o
    0x00014528   0x00014528   0x000002ac   Code   RO          903    i.app_tp_screen_analysis_int  WL568_S21_NT37701_TP.lib(app_tp_for_custom_s8.o)
    0x000147d4   0x000147d4   0x00000030   Code   RO          264    i.app_tp_screen_init  app_tp_transfer.o
    0x00014804   0x00014804   0x0000000c   Code   RO          265    i.app_tp_screen_int_callback  app_tp_transfer.o
    0x00014810   0x00014810   0x00000040   Code   RO          266    i.app_tp_transfer_screen_const  app_tp_transfer.o
    0x00014850   0x00014850   0x00000138   Code   RO          267    i.app_tp_transfer_screen_int  app_tp_transfer.o
    0x00014988   0x00014988   0x00000018   Code   RO          268    i.app_tp_transfer_screen_start  app_tp_transfer.o
    0x000149a0   0x000149a0   0x00000024   Code   RO          506    i.board_Init        board.o
    0x000149c4   0x000149c4   0x000003cc   Code   RO         1694    i.calc_framebuffer_setting  CVWL568.lib(hal_internal_vsync.o)
    0x00014d90   0x00014d90   0x000000c8   Code   RO         2622    i.ceil              m_ps.l(ceil.o)
    0x00014e58   0x00014e58   0x0000002c   Code   RO         1695    i.check_mipi_rx_tx_video_info  CVWL568.lib(hal_internal_vsync.o)
    0x00014e84   0x00014e84   0x00000094   Code   RO         1696    i.check_pkt_buf_rev  CVWL568.lib(hal_internal_vsync.o)
    0x00014f18   0x00014f18   0x00000058   Code   RO         1766    i.dcs_packet_fifo_alloc  CVWL568.lib(dcs_packet_fifo.o)
    0x00014f70   0x00014f70   0x00000018   Code   RO         1767    i.dcs_packet_fifo_init  CVWL568.lib(dcs_packet_fifo.o)
    0x00014f88   0x00014f88   0x00000044   Code   RO         1768    i.dcs_packet_free_fifo_header  CVWL568.lib(dcs_packet_fifo.o)
    0x00014fcc   0x00014fcc   0x00000024   Code   RO         1769    i.dcs_packet_get_fifo_header  CVWL568.lib(dcs_packet_fifo.o)
    0x00014ff0   0x00014ff0   0x0000001c   Code   RO         1697    i.dcs_sw_filter     CVWL568.lib(hal_internal_vsync.o)
    0x0001500c   0x0001500c   0x00000018   Code   RO          882    i.delayMs           CVWL568.lib(tau_delay.o)
    0x00015024   0x00015024   0x00000022   Code   RO          883    i.delayUs           CVWL568.lib(tau_delay.o)
    0x00015046   0x00015046   0x00000002   PAD
    0x00015048   0x00015048   0x00000038   Code   RO         1621    i.drv_ap_rst_trig_edge_detect  CVWL568.lib(drv_sys_cfg.o)
    0x00015080   0x00015080   0x0000000c   Code   RO         2308    i.drv_chip_info_get_info  CVWL568.lib(drv_chip_info.o)
    0x0001508c   0x0001508c   0x00000040   Code   RO         2309    i.drv_chip_info_init  CVWL568.lib(drv_chip_info.o)
    0x000150cc   0x000150cc   0x000000c8   Code   RO         2310    i.drv_chip_rx_info_check  CVWL568.lib(drv_chip_info.o)
    0x00015194   0x00015194   0x00000014   Code   RO         2311    i.drv_chip_rx_init_done  CVWL568.lib(drv_chip_info.o)
    0x000151a8   0x000151a8   0x00000058   Code   RO         1137    i.drv_common_enable_systick  CVWL568.lib(drv_common.o)
    0x00015200   0x00015200   0x00000008   Code   RO         1140    i.drv_common_system_init  CVWL568.lib(drv_common.o)
    0x00015208   0x00015208   0x00000010   Code   RO         1161    i.drv_crgu_config_reset_modules  CVWL568.lib(drv_crgu.o)
    0x00015218   0x00015218   0x00000014   Code   RO         1173    i.drv_crgu_set_ahb_pre_div  CVWL568.lib(drv_crgu.o)
    0x0001522c   0x0001522c   0x00000014   Code   RO         1174    i.drv_crgu_set_ahb_src  CVWL568.lib(drv_crgu.o)
    0x00015240   0x00015240   0x00000020   Code   RO         1177    i.drv_crgu_set_clock  CVWL568.lib(drv_crgu.o)
    0x00015260   0x00015260   0x00000014   Code   RO         1178    i.drv_crgu_set_dpi_mux_src  CVWL568.lib(drv_crgu.o)
    0x00015274   0x00015274   0x00000018   Code   RO         1179    i.drv_crgu_set_dpi_pre_div  CVWL568.lib(drv_crgu.o)
    0x0001528c   0x0001528c   0x00000014   Code   RO         1180    i.drv_crgu_set_dpi_pre_src  CVWL568.lib(drv_crgu.o)
    0x000152a0   0x000152a0   0x00000014   Code   RO         1181    i.drv_crgu_set_dsc_core_div  CVWL568.lib(drv_crgu.o)
    0x000152b4   0x000152b4   0x00000014   Code   RO         1182    i.drv_crgu_set_dsco_src  CVWL568.lib(drv_crgu.o)
    0x000152c8   0x000152c8   0x00000014   Code   RO         1183    i.drv_crgu_set_dsco_src_div  CVWL568.lib(drv_crgu.o)
    0x000152dc   0x000152dc   0x00000014   Code   RO         1184    i.drv_crgu_set_fb_div  CVWL568.lib(drv_crgu.o)
    0x000152f0   0x000152f0   0x00000014   Code   RO         1185    i.drv_crgu_set_fb_src  CVWL568.lib(drv_crgu.o)
    0x00015304   0x00015304   0x00000014   Code   RO         1188    i.drv_crgu_set_lcdc_div  CVWL568.lib(drv_crgu.o)
    0x00015318   0x00015318   0x00000014   Code   RO         1189    i.drv_crgu_set_lcdc_src  CVWL568.lib(drv_crgu.o)
    0x0001532c   0x0001532c   0x00000014   Code   RO         1190    i.drv_crgu_set_mipi_cfg_src  CVWL568.lib(drv_crgu.o)
    0x00015340   0x00015340   0x00000018   Code   RO         1191    i.drv_crgu_set_mipi_ref_src  CVWL568.lib(drv_crgu.o)
    0x00015358   0x00015358   0x00000018   Code   RO         1194    i.drv_crgu_set_reset  CVWL568.lib(drv_crgu.o)
    0x00015370   0x00015370   0x00000014   Code   RO         1195    i.drv_crgu_set_rxbr_div  CVWL568.lib(drv_crgu.o)
    0x00015384   0x00015384   0x00000014   Code   RO         1196    i.drv_crgu_set_rxbr_src  CVWL568.lib(drv_crgu.o)
    0x00015398   0x00015398   0x00000014   Code   RO         1198    i.drv_crgu_set_vidc_src  CVWL568.lib(drv_crgu.o)
    0x000153ac   0x000153ac   0x00000018   Code   RO         1250    i.drv_dma_clear_flag  CVWL568.lib(drv_dma.o)
    0x000153c4   0x000153c4   0x0000001c   Code   RO         1251    i.drv_dma_create_handle  CVWL568.lib(drv_dma.o)
    0x000153e0   0x000153e0   0x00000010   Code   RO         1253    i.drv_dma_disenable_channel  CVWL568.lib(drv_dma.o)
    0x000153f0   0x000153f0   0x00000010   Code   RO         1255    i.drv_dma_enable_channel  CVWL568.lib(drv_dma.o)
    0x00015400   0x00015400   0x00000024   Code   RO         1256    i.drv_dma_enable_channel_interrupts  CVWL568.lib(drv_dma.o)
    0x00015424   0x00015424   0x0000000c   Code   RO         1258    i.drv_dma_get_channel_flag  CVWL568.lib(drv_dma.o)
    0x00015430   0x00015430   0x00000090   Code   RO         1261    i.drv_dma_irq_handler  CVWL568.lib(drv_dma.o)
    0x000154c0   0x000154c0   0x00000012   Code   RO         1263    i.drv_dma_prepar_transfer  CVWL568.lib(drv_dma.o)
    0x000154d2   0x000154d2   0x0000001a   Code   RO         1265    i.drv_dma_set_burst  CVWL568.lib(drv_dma.o)
    0x000154ec   0x000154ec   0x00000006   Code   RO         1266    i.drv_dma_set_callback  CVWL568.lib(drv_dma.o)
    0x000154f2   0x000154f2   0x00000002   PAD
    0x000154f4   0x000154f4   0x00000044   Code   RO         1268    i.drv_dma_set_transfer  CVWL568.lib(drv_dma.o)
    0x00015538   0x00015538   0x00000036   Code   RO         2321    i.drv_dsc_dec_convert_pps_rc_parameter  CVWL568.lib(drv_dsc_dec.o)
    0x0001556e   0x0001556e   0x0000000c   Code   RO         2322    i.drv_dsc_dec_disable  CVWL568.lib(drv_dsc_dec.o)
    0x0001557a   0x0001557a   0x00000002   PAD
    0x0001557c   0x0001557c   0x00000074   Code   RO         2323    i.drv_dsc_dec_enable  CVWL568.lib(drv_dsc_dec.o)
    0x000155f0   0x000155f0   0x0000000a   Code   RO         2324    i.drv_dsc_dec_get_nslc  CVWL568.lib(drv_dsc_dec.o)
    0x000155fa   0x000155fa   0x00000028   Code   RO         2326    i.drv_dsc_dec_set_u8_pps  CVWL568.lib(drv_dsc_dec.o)
    0x00015622   0x00015622   0x00000002   PAD
    0x00015624   0x00015624   0x00000104   Code   RO         1780    i.drv_dsi_rx_calc_ipi_tx_delay  CVWL568.lib(drv_dsi_rx.o)
    0x00015728   0x00015728   0x00000040   Code   RO         1781    i.drv_dsi_rx_enable_irq  CVWL568.lib(drv_dsi_rx.o)
    0x00015768   0x00015768   0x00000050   Code   RO         1782    i.drv_dsi_rx_get_color_bpp  CVWL568.lib(drv_dsi_rx.o)
    0x000157b8   0x000157b8   0x0000001c   Code   RO         1783    i.drv_dsi_rx_get_color_pcc  CVWL568.lib(drv_dsi_rx.o)
    0x000157d4   0x000157d4   0x00000008   Code   RO         1784    i.drv_dsi_rx_get_compression_en  CVWL568.lib(drv_dsi_rx.o)
    0x000157dc   0x000157dc   0x00000006   Code   RO         1785    i.drv_dsi_rx_get_max_ret_size  CVWL568.lib(drv_dsi_rx.o)
    0x000157e2   0x000157e2   0x0000000e   Code   RO         1789    i.drv_dsi_rx_power_up  CVWL568.lib(drv_dsi_rx.o)
    0x000157f0   0x000157f0   0x00000020   Code   RO         1790    i.drv_dsi_rx_set_ctrl_cfg  CVWL568.lib(drv_dsi_rx.o)
    0x00015810   0x00015810   0x00000010   Code   RO         1791    i.drv_dsi_rx_set_ddi_cfg  CVWL568.lib(drv_dsi_rx.o)
    0x00015820   0x00015820   0x00000004   Code   RO         1793    i.drv_dsi_rx_set_inten  CVWL568.lib(drv_dsi_rx.o)
    0x00015824   0x00015824   0x00000010   Code   RO         1794    i.drv_dsi_rx_set_ipi_cfg  CVWL568.lib(drv_dsi_rx.o)
    0x00015834   0x00015834   0x00000046   Code   RO         1796    i.drv_dsi_rx_set_lane_swap  CVWL568.lib(drv_dsi_rx.o)
    0x0001587a   0x0001587a   0x00000026   Code   RO         1797    i.drv_dsi_rx_set_resp_cnt  CVWL568.lib(drv_dsi_rx.o)
    0x000158a0   0x000158a0   0x000000f0   Code   RO         1798    i.drv_dsi_rx_set_up_phy  CVWL568.lib(drv_dsi_rx.o)
    0x00015990   0x00015990   0x0000000e   Code   RO         1799    i.drv_dsi_rx_shut_down  CVWL568.lib(drv_dsi_rx.o)
    0x0001599e   0x0001599e   0x00000014   Code   RO         1837    i.drv_dsi_tx_command_header  CVWL568.lib(drv_dsi_tx.o)
    0x000159b2   0x000159b2   0x0000006c   Code   RO         1838    i.drv_dsi_tx_command_mode_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x00015a1e   0x00015a1e   0x00000004   Code   RO         1839    i.drv_dsi_tx_command_put_payload  CVWL568.lib(drv_dsi_tx.o)
    0x00015a22   0x00015a22   0x00000018   Code   RO         1840    i.drv_dsi_tx_config_eotp  CVWL568.lib(drv_dsi_tx.o)
    0x00015a3a   0x00015a3a   0x00000008   Code   RO         1841    i.drv_dsi_tx_config_int  CVWL568.lib(drv_dsi_tx.o)
    0x00015a42   0x00015a42   0x00000008   Code   RO         1842    i.drv_dsi_tx_dpi_lpcmd_time  CVWL568.lib(drv_dsi_tx.o)
    0x00015a4a   0x00015a4a   0x0000000a   Code   RO         1843    i.drv_dsi_tx_dpi_mode  CVWL568.lib(drv_dsi_tx.o)
    0x00015a54   0x00015a54   0x00000024   Code   RO         1844    i.drv_dsi_tx_dpi_polarity  CVWL568.lib(drv_dsi_tx.o)
    0x00015a78   0x00015a78   0x00000004   Code   RO         1845    i.drv_dsi_tx_edpi_cmd_size  CVWL568.lib(drv_dsi_tx.o)
    0x00015a7c   0x00015a7c   0x00000004   Code   RO         1847    i.drv_dsi_tx_get_cmd_status  CVWL568.lib(drv_dsi_tx.o)
    0x00015a80   0x00015a80   0x00000004   Code   RO         1849    i.drv_dsi_tx_mode   CVWL568.lib(drv_dsi_tx.o)
    0x00015a84   0x00015a84   0x00000018   Code   RO         1850    i.drv_dsi_tx_phy_clock_lane_auto_lp  CVWL568.lib(drv_dsi_tx.o)
    0x00015a9c   0x00015a9c   0x0000001a   Code   RO         1851    i.drv_dsi_tx_phy_clock_lane_req_hs  CVWL568.lib(drv_dsi_tx.o)
    0x00015ab6   0x00015ab6   0x0000000c   Code   RO         1853    i.drv_dsi_tx_phy_lane_mode  CVWL568.lib(drv_dsi_tx.o)
    0x00015ac2   0x00015ac2   0x00000064   Code   RO         1857    i.drv_dsi_tx_phy_status_ready  CVWL568.lib(drv_dsi_tx.o)
    0x00015b26   0x00015b26   0x0000003e   Code   RO         1858    i.drv_dsi_tx_phy_status_stopstate  CVWL568.lib(drv_dsi_tx.o)
    0x00015b64   0x00015b64   0x0000010c   Code   RO         1860    i.drv_dsi_tx_phy_test_setup  CVWL568.lib(drv_dsi_tx.o)
    0x00015c70   0x00015c70   0x0000001e   Code   RO         1861    i.drv_dsi_tx_phy_time_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x00015c8e   0x00015c8e   0x00000008   Code   RO         1865    i.drv_dsi_tx_powerup  CVWL568.lib(drv_dsi_tx.o)
    0x00015c96   0x00015c96   0x0000001c   Code   RO         1866    i.drv_dsi_tx_response_mode  CVWL568.lib(drv_dsi_tx.o)
    0x00015cb2   0x00015cb2   0x00000018   Code   RO         1869    i.drv_dsi_tx_set_bta_ack  CVWL568.lib(drv_dsi_tx.o)
    0x00015cca   0x00015cca   0x0000000c   Code   RO         1870    i.drv_dsi_tx_set_esc_div  CVWL568.lib(drv_dsi_tx.o)
    0x00015cd6   0x00015cd6   0x00000002   PAD
    0x00015cd8   0x00015cd8   0x00000034   Code   RO         1871    i.drv_dsi_tx_set_int  CVWL568.lib(drv_dsi_tx.o)
    0x00015d0c   0x00015d0c   0x00000010   Code   RO         1872    i.drv_dsi_tx_set_time_out_div  CVWL568.lib(drv_dsi_tx.o)
    0x00015d1c   0x00015d1c   0x00000008   Code   RO         1873    i.drv_dsi_tx_set_video_chunk  CVWL568.lib(drv_dsi_tx.o)
    0x00015d24   0x00015d24   0x00000022   Code   RO         1874    i.drv_dsi_tx_set_video_timing  CVWL568.lib(drv_dsi_tx.o)
    0x00015d46   0x00015d46   0x00000008   Code   RO         1876    i.drv_dsi_tx_shutdown  CVWL568.lib(drv_dsi_tx.o)
    0x00015d4e   0x00015d4e   0x00000026   Code   RO         1877    i.drv_dsi_tx_timeout_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x00015d74   0x00015d74   0x000000aa   Code   RO         1880    i.drv_dsi_tx_video_mode_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x00015e1e   0x00015e1e   0x00000016   Code   RO         1881    i.drv_dsi_tx_video_mode_disable_hact_cmd  CVWL568.lib(drv_dsi_tx.o)
    0x00015e34   0x00015e34   0x00000018   Code   RO         1882    i.drv_dsi_tx_video_mode_set_lp_cmd  CVWL568.lib(drv_dsi_tx.o)
    0x00015e4c   0x00015e4c   0x00000020   Code   RO         2602    i.drv_efuse_enter_inactive  CVWL568.lib(drv_efuse.o)
    0x00015e6c   0x00015e6c   0x0000000c   Code   RO         2605    i.drv_efuse_int_enable  CVWL568.lib(drv_efuse.o)
    0x00015e78   0x00015e78   0x00000032   Code   RO         2606    i.drv_efuse_read    CVWL568.lib(drv_efuse.o)
    0x00015eaa   0x00015eaa   0x00000018   Code   RO         2607    i.drv_efuse_read_req  CVWL568.lib(drv_efuse.o)
    0x00015ec2   0x00015ec2   0x00000002   PAD
    0x00015ec4   0x00015ec4   0x00000018   Code   RO         1393    i.drv_gpio_get_input_data  CVWL568.lib(drv_gpio.o)
    0x00015edc   0x00015edc   0x0000000c   Code   RO         1395    i.drv_gpio_register_ap_reset_callback  CVWL568.lib(drv_gpio.o)
    0x00015ee8   0x00015ee8   0x00000014   Code   RO         1396    i.drv_gpio_register_callback  CVWL568.lib(drv_gpio.o)
    0x00015efc   0x00015efc   0x00000044   Code   RO         1398    i.drv_gpio_set_int  CVWL568.lib(drv_gpio.o)
    0x00015f40   0x00015f40   0x00000020   Code   RO         1399    i.drv_gpio_set_ioe  CVWL568.lib(drv_gpio.o)
    0x00015f60   0x00015f60   0x00000010   Code   RO         1400    i.drv_gpio_set_mode0  CVWL568.lib(drv_gpio.o)
    0x00015f70   0x00015f70   0x00000010   Code   RO         1401    i.drv_gpio_set_mode1  CVWL568.lib(drv_gpio.o)
    0x00015f80   0x00015f80   0x00000010   Code   RO         1402    i.drv_gpio_set_mode2  CVWL568.lib(drv_gpio.o)
    0x00015f90   0x00015f90   0x00000010   Code   RO         1403    i.drv_gpio_set_mode3  CVWL568.lib(drv_gpio.o)
    0x00015fa0   0x00015fa0   0x00000020   Code   RO          716    i.drv_gpio_set_output_data  CVWL568.lib(hal_gpio.o)
    0x00015fc0   0x00015fc0   0x00000130   Code   RO         1404    i.drv_gpio_set_pull_state  CVWL568.lib(drv_gpio.o)
    0x000160f0   0x000160f0   0x00000034   Code   RO         1436    i.drv_i2c_dma_callback  CVWL568.lib(drv_i2c_dma.o)
    0x00016124   0x00016124   0x000000ac   Code   RO         1437    i.drv_i2c_dma_init  CVWL568.lib(drv_i2c_dma.o)
    0x000161d0   0x000161d0   0x0000001a   Code   RO         1438    i.drv_i2c_enable_rx_dma  CVWL568.lib(drv_i2c_dma.o)
    0x000161ea   0x000161ea   0x00000018   Code   RO         1439    i.drv_i2c_enable_tx_dma  CVWL568.lib(drv_i2c_dma.o)
    0x00016202   0x00016202   0x00000002   PAD
    0x00016204   0x00016204   0x00000060   Code   RO         1463    i.drv_i2c_m_clear_it_pending_bit  CVWL568.lib(drv_i2c_master.o)
    0x00016264   0x00016264   0x00000010   Code   RO         1465    i.drv_i2c_m_enable  CVWL568.lib(drv_i2c_master.o)
    0x00016274   0x00016274   0x00000038   Code   RO         1466    i.drv_i2c_m_enable_intr  CVWL568.lib(drv_i2c_master.o)
    0x000162ac   0x000162ac   0x0000000c   Code   RO         1469    i.drv_i2c_m_set_callback  CVWL568.lib(drv_i2c_master.o)
    0x000162b8   0x000162b8   0x0000008c   Code   RO         1473    i.drv_i2c_master_init  CVWL568.lib(drv_i2c_master.o)
    0x00016344   0x00016344   0x0000005c   Code   RO         1440    i.drv_i2c_master_read_dma  CVWL568.lib(drv_i2c_dma.o)
    0x000163a0   0x000163a0   0x0000003c   Code   RO         1441    i.drv_i2c_master_write_dma  CVWL568.lib(drv_i2c_dma.o)
    0x000163dc   0x000163dc   0x0000002e   Code   RO         1442    i.drv_i2c_master_write_read_cmd  CVWL568.lib(drv_i2c_dma.o)
    0x0001640a   0x0001640a   0x00000002   PAD
    0x0001640c   0x0001640c   0x0000005c   Code   RO         1496    i.drv_i2c_s_clear_it_pending_bit  CVWL568.lib(drv_i2c_slave.o)
    0x00016468   0x00016468   0x00000034   Code   RO         1499    i.drv_i2c_s_enable_intr  CVWL568.lib(drv_i2c_slave.o)
    0x0001649c   0x0001649c   0x0000001c   Code   RO         1500    i.drv_i2c_s_get_fifo_status  CVWL568.lib(drv_i2c_slave.o)
    0x000164b8   0x000164b8   0x0000000c   Code   RO         1503    i.drv_i2c_s_set_callback  CVWL568.lib(drv_i2c_slave.o)
    0x000164c4   0x000164c4   0x00000020   Code   RO         1506    i.drv_i2c_s_write_data  CVWL568.lib(drv_i2c_slave.o)
    0x000164e4   0x000164e4   0x00000058   Code   RO         1443    i.drv_i2c_set_dma_irq_callback  CVWL568.lib(drv_i2c_dma.o)
    0x0001653c   0x0001653c   0x00000044   Code   RO         1507    i.drv_i2c_slave_init  CVWL568.lib(drv_i2c_slave.o)
    0x00016580   0x00016580   0x0000001c   Code   RO         1444    i.drv_i2c_slave_write_dma  CVWL568.lib(drv_i2c_dma.o)
    0x0001659c   0x0001659c   0x00000018   Code   RO         1949    i.drv_lcdc_config_bypass  CVWL568.lib(drv_lcdc.o)
    0x000165b4   0x000165b4   0x00000030   Code   RO         1950    i.drv_lcdc_config_ccm  CVWL568.lib(drv_lcdc.o)
    0x000165e4   0x000165e4   0x00000016   Code   RO         1951    i.drv_lcdc_config_disp_mode  CVWL568.lib(drv_lcdc.o)
    0x000165fa   0x000165fa   0x00000024   Code   RO         1952    i.drv_lcdc_config_dpi_polarity  CVWL568.lib(drv_lcdc.o)
    0x0001661e   0x0001661e   0x00000026   Code   RO         1953    i.drv_lcdc_config_dpi_timing  CVWL568.lib(drv_lcdc.o)
    0x00016644   0x00016644   0x00000016   Code   RO         1954    i.drv_lcdc_config_edpi_mode  CVWL568.lib(drv_lcdc.o)
    0x0001665a   0x0001665a   0x00000016   Code   RO         1955    i.drv_lcdc_config_endianness  CVWL568.lib(drv_lcdc.o)
    0x00016670   0x00016670   0x0000000c   Code   RO         1956    i.drv_lcdc_config_input_size  CVWL568.lib(drv_lcdc.o)
    0x0001667c   0x0001667c   0x0000001e   Code   RO         1957    i.drv_lcdc_config_int  CVWL568.lib(drv_lcdc.o)
    0x0001669a   0x0001669a   0x00000022   Code   RO         1958    i.drv_lcdc_config_int_single  CVWL568.lib(drv_lcdc.o)
    0x000166bc   0x000166bc   0x00000022   Code   RO         1959    i.drv_lcdc_config_overwrite  CVWL568.lib(drv_lcdc.o)
    0x000166de   0x000166de   0x0000000c   Code   RO         1960    i.drv_lcdc_config_overwrite_rgb  CVWL568.lib(drv_lcdc.o)
    0x000166ea   0x000166ea   0x0000001a   Code   RO         1961    i.drv_lcdc_config_partial_display_area  CVWL568.lib(drv_lcdc.o)
    0x00016704   0x00016704   0x00000022   Code   RO         1962    i.drv_lcdc_config_partial_display_enable  CVWL568.lib(drv_lcdc.o)
    0x00016726   0x00016726   0x0000001a   Code   RO         1964    i.drv_lcdc_config_scale_up_coef  CVWL568.lib(drv_lcdc.o)
    0x00016740   0x00016740   0x0000000c   Code   RO         1965    i.drv_lcdc_config_scale_up_step  CVWL568.lib(drv_lcdc.o)
    0x0001674c   0x0001674c   0x0000004c   Code   RO         1966    i.drv_lcdc_config_src_parameter  CVWL568.lib(drv_lcdc.o)
    0x00016798   0x00016798   0x00000006   Code   RO         1967    i.drv_lcdc_config_thresh  CVWL568.lib(drv_lcdc.o)
    0x0001679e   0x0001679e   0x00000012   Code   RO         1968    i.drv_lcdc_ctrl_flow  CVWL568.lib(drv_lcdc.o)
    0x000167b0   0x000167b0   0x00000020   Code   RO         1970    i.drv_lcdc_enable_shadow_reg  CVWL568.lib(drv_lcdc.o)
    0x000167d0   0x000167d0   0x00000034   Code   RO         1971    i.drv_lcdc_set_int  CVWL568.lib(drv_lcdc.o)
    0x00016804   0x00016804   0x00000014   Code   RO         1973    i.drv_lcdc_set_video_hw_mode  CVWL568.lib(drv_lcdc.o)
    0x00016818   0x00016818   0x00000020   Code   RO         1974    i.drv_lcdc_start    CVWL568.lib(drv_lcdc.o)
    0x00016838   0x00016838   0x0000000c   Code   RO         2008    i.drv_memc_clear_status  CVWL568.lib(drv_memc.o)
    0x00016844   0x00016844   0x00000040   Code   RO         2009    i.drv_memc_enable_irq  CVWL568.lib(drv_memc.o)
    0x00016884   0x00016884   0x0000000c   Code   RO         2010    i.drv_memc_gen_a_tear_signal  CVWL568.lib(drv_memc.o)
    0x00016890   0x00016890   0x00000012   Code   RO         2011    i.drv_memc_get_status  CVWL568.lib(drv_memc.o)
    0x000168a2   0x000168a2   0x00000010   Code   RO         2012    i.drv_memc_rate_transfer_sel  CVWL568.lib(drv_memc.o)
    0x000168b2   0x000168b2   0x0000000e   Code   RO         2013    i.drv_memc_sel_vsync  CVWL568.lib(drv_memc.o)
    0x000168c0   0x000168c0   0x00000014   Code   RO         2014    i.drv_memc_set_active_height  CVWL568.lib(drv_memc.o)
    0x000168d4   0x000168d4   0x0000000c   Code   RO         2015    i.drv_memc_set_data_mode  CVWL568.lib(drv_memc.o)
    0x000168e0   0x000168e0   0x00000010   Code   RO         2018    i.drv_memc_set_double_buffer  CVWL568.lib(drv_memc.o)
    0x000168f0   0x000168f0   0x00000012   Code   RO         2019    i.drv_memc_set_double_buffer_reverse  CVWL568.lib(drv_memc.o)
    0x00016902   0x00016902   0x00000010   Code   RO         2021    i.drv_memc_set_fs_en_conditions  CVWL568.lib(drv_memc.o)
    0x00016912   0x00016912   0x00000014   Code   RO         2022    i.drv_memc_set_inten  CVWL568.lib(drv_memc.o)
    0x00016926   0x00016926   0x00000002   PAD
    0x00016928   0x00016928   0x00000018   Code   RO         2023    i.drv_memc_set_lcdc_st_conditions  CVWL568.lib(drv_memc.o)
    0x00016940   0x00016940   0x0000001a   Code   RO         2024    i.drv_memc_set_ltpo_mode  CVWL568.lib(drv_memc.o)
    0x0001695a   0x0001695a   0x0000000e   Code   RO         2028    i.drv_memc_set_tear_mode  CVWL568.lib(drv_memc.o)
    0x00016968   0x00016968   0x00000028   Code   RO         2029    i.drv_memc_set_tear_waveform  CVWL568.lib(drv_memc.o)
    0x00016990   0x00016990   0x0000000e   Code   RO         2031    i.drv_memc_set_vidc_sync_cnt  CVWL568.lib(drv_memc.o)
    0x0001699e   0x0001699e   0x00000002   PAD
    0x000169a0   0x000169a0   0x00000008   Code   RO         1528    i.drv_param_init_get_ccm  CVWL568.lib(drv_param_init.o)
    0x000169a8   0x000169a8   0x00000014   Code   RO         1529    i.drv_param_init_get_scld_filter_h  CVWL568.lib(drv_param_init.o)
    0x000169bc   0x000169bc   0x00000014   Code   RO         1530    i.drv_param_init_get_scld_filter_v  CVWL568.lib(drv_param_init.o)
    0x000169d0   0x000169d0   0x00000008   Code   RO         1531    i.drv_param_init_get_sclu_filter  CVWL568.lib(drv_param_init.o)
    0x000169d8   0x000169d8   0x00000014   Code   RO         1532    i.drv_param_init_set_ccm  CVWL568.lib(drv_param_init.o)
    0x000169ec   0x000169ec   0x00000064   Code   RO         1533    i.drv_param_init_set_scld_filter  CVWL568.lib(drv_param_init.o)
    0x00016a50   0x00016a50   0x00000024   Code   RO         1535    i.drv_param_p2r_filter_init  CVWL568.lib(drv_param_init.o)
    0x00016a74   0x00016a74   0x00000010   Code   RO         2280    i.drv_phy_enable_calibration  CVWL568.lib(drv_phy_common.o)
    0x00016a84   0x00016a84   0x0000003c   Code   RO         2281    i.drv_phy_get_calibration  CVWL568.lib(drv_phy_common.o)
    0x00016ac0   0x00016ac0   0x00000060   Code   RO         2282    i.drv_phy_get_pll_para  CVWL568.lib(drv_phy_common.o)
    0x00016b20   0x00016b20   0x00000054   Code   RO         2283    i.drv_phy_get_rate_para  CVWL568.lib(drv_phy_common.o)
    0x00016b74   0x00016b74   0x00000010   Code   RO         2284    i.drv_phy_test_clear  CVWL568.lib(drv_phy_common.o)
    0x00016b84   0x00016b84   0x00000018   Code   RO         2285    i.drv_phy_test_lock  CVWL568.lib(drv_phy_common.o)
    0x00016b9c   0x00016b9c   0x00000020   Code   RO         2287    i.drv_phy_test_write_1_byte  CVWL568.lib(drv_phy_common.o)
    0x00016bbc   0x00016bbc   0x00000026   Code   RO         2288    i.drv_phy_test_write_2_byte  CVWL568.lib(drv_phy_common.o)
    0x00016be2   0x00016be2   0x0000001e   Code   RO         2289    i.drv_phy_test_write_code  CVWL568.lib(drv_phy_common.o)
    0x00016c00   0x00016c00   0x00000020   Code   RO         2290    i.drv_phy_test_write_data  CVWL568.lib(drv_phy_common.o)
    0x00016c20   0x00016c20   0x00000020   Code   RO         1551    i.drv_pwr_set_cp_mode  CVWL568.lib(drv_pwr.o)
    0x00016c40   0x00016c40   0x00000018   Code   RO         1552    i.drv_pwr_set_pvd_mode  CVWL568.lib(drv_pwr.o)
    0x00016c58   0x00016c58   0x00000030   Code   RO         1553    i.drv_pwr_set_system_clk_src  CVWL568.lib(drv_pwr.o)
    0x00016c88   0x00016c88   0x0000000c   Code   RO         1800    i.drv_rx_phy_test_clear  CVWL568.lib(drv_dsi_rx.o)
    0x00016c94   0x00016c94   0x00000010   Code   RO         1801    i.drv_rx_phy_test_lock  CVWL568.lib(drv_dsi_rx.o)
    0x00016ca4   0x00016ca4   0x00000014   Code   RO         1803    i.drv_rx_phy_test_write_1_byte  CVWL568.lib(drv_dsi_rx.o)
    0x00016cb8   0x00016cb8   0x00000016   Code   RO         1804    i.drv_rx_phy_test_write_2_byte  CVWL568.lib(drv_dsi_rx.o)
    0x00016cce   0x00016cce   0x0000000a   Code   RO         2067    i.drv_rxbr_clear_pkt_buffer  CVWL568.lib(drv_rxbr.o)
    0x00016cd8   0x00016cd8   0x00000004   Code   RO         2068    i.drv_rxbr_clear_status0  CVWL568.lib(drv_rxbr.o)
    0x00016cdc   0x00016cdc   0x0000005a   Code   RO         2070    i.drv_rxbr_enable_irq  CVWL568.lib(drv_rxbr.o)
    0x00016d36   0x00016d36   0x00000002   PAD
    0x00016d38   0x00016d38   0x00000014   Code   RO         2071    i.drv_rxbr_frame_drop_cfg  CVWL568.lib(drv_rxbr.o)
    0x00016d4c   0x00016d4c   0x0000003c   Code   RO         2072    i.drv_rxbr_get_clk  CVWL568.lib(drv_rxbr.o)
    0x00016d88   0x00016d88   0x00000004   Code   RO         2073    i.drv_rxbr_get_col_addr  CVWL568.lib(drv_rxbr.o)
    0x00016d8c   0x00016d8c   0x00000012   Code   RO         1698    i.drv_rxbr_get_int_source  CVWL568.lib(hal_internal_vsync.o)
    0x00016d9e   0x00016d9e   0x00000004   Code   RO         2076    i.drv_rxbr_get_page_addr  CVWL568.lib(drv_rxbr.o)
    0x00016da2   0x00016da2   0x00000012   Code   RO         1699    i.drv_rxbr_get_status0  CVWL568.lib(hal_internal_vsync.o)
    0x00016db4   0x00016db4   0x0000000c   Code   RO         2078    i.drv_rxbr_hline_rcv0_cfg  CVWL568.lib(drv_rxbr.o)
    0x00016dc0   0x00016dc0   0x00000008   Code   RO         2079    i.drv_rxbr_hline_rcv_cfg  CVWL568.lib(drv_rxbr.o)
    0x00016dc8   0x00016dc8   0x0000000c   Code   RO         2080    i.drv_rxbr_register_irq0_callback  CVWL568.lib(drv_rxbr.o)
    0x00016dd4   0x00016dd4   0x0000000c   Code   RO         2081    i.drv_rxbr_register_irq1_callback  CVWL568.lib(drv_rxbr.o)
    0x00016de0   0x00016de0   0x00000014   Code   RO         2082    i.drv_rxbr_set_ack_pkt_header  CVWL568.lib(drv_rxbr.o)
    0x00016df4   0x00016df4   0x000000cc   Code   RO         2083    i.drv_rxbr_set_cmd_filter  CVWL568.lib(drv_rxbr.o)
    0x00016ec0   0x00016ec0   0x00000014   Code   RO         2085    i.drv_rxbr_set_color_format  CVWL568.lib(drv_rxbr.o)
    0x00016ed4   0x00016ed4   0x00000014   Code   RO         2087    i.drv_rxbr_set_inten  CVWL568.lib(drv_rxbr.o)
    0x00016ee8   0x00016ee8   0x00000010   Code   RO         2088    i.drv_rxbr_set_ltpo_drop_th  CVWL568.lib(drv_rxbr.o)
    0x00016ef8   0x00016ef8   0x00000026   Code   RO         2090    i.drv_rxbr_set_usr_cfg  CVWL568.lib(drv_rxbr.o)
    0x00016f1e   0x00016f1e   0x00000008   Code   RO         2091    i.drv_rxbr_set_usr_col  CVWL568.lib(drv_rxbr.o)
    0x00016f26   0x00016f26   0x00000008   Code   RO         2092    i.drv_rxbr_set_usr_row  CVWL568.lib(drv_rxbr.o)
    0x00016f2e   0x00016f2e   0x00000002   PAD
    0x00016f30   0x00016f30   0x00000020   Code   RO         1597    i.drv_spi_m_read_data  CVWL568.lib(drv_spi_master.o)
    0x00016f50   0x00016f50   0x00000048   Code   RO         2474    i.drv_swire_set_int  CVWL568.lib(drv_swire.o)
    0x00016f98   0x00016f98   0x0000000c   Code   RO         1622    i.drv_sys_cfg_clear_all_int  CVWL568.lib(drv_sys_cfg.o)
    0x00016fa4   0x00016fa4   0x00000028   Code   RO         1623    i.drv_sys_cfg_clear_pending  CVWL568.lib(drv_sys_cfg.o)
    0x00016fcc   0x00016fcc   0x00000018   Code   RO         1626    i.drv_sys_cfg_sel_ap_rst_lvl_trig  CVWL568.lib(drv_sys_cfg.o)
    0x00016fe4   0x00016fe4   0x0000001c   Code   RO         1627    i.drv_sys_cfg_sel_ap_rst_trig  CVWL568.lib(drv_sys_cfg.o)
    0x00017000   0x00017000   0x00000024   Code   RO         1628    i.drv_sys_cfg_sel_gpio_group  CVWL568.lib(drv_sys_cfg.o)
    0x00017024   0x00017024   0x00000024   Code   RO         1629    i.drv_sys_cfg_sel_int_trig  CVWL568.lib(drv_sys_cfg.o)
    0x00017048   0x00017048   0x00000010   Code   RO         1631    i.drv_sys_cfg_set_dma_rx_req  CVWL568.lib(drv_sys_cfg.o)
    0x00017058   0x00017058   0x00000010   Code   RO         1632    i.drv_sys_cfg_set_dma_tx_req  CVWL568.lib(drv_sys_cfg.o)
    0x00017068   0x00017068   0x00000024   Code   RO         1633    i.drv_sys_cfg_set_int  CVWL568.lib(drv_sys_cfg.o)
    0x0001708c   0x0001708c   0x0000001a   Code   RO         1657    i.drv_timer_clear_status_flags  CVWL568.lib(drv_timer.o)
    0x000170a6   0x000170a6   0x00000020   Code   RO         1658    i.drv_timer_enable  CVWL568.lib(drv_timer.o)
    0x000170c6   0x000170c6   0x00000002   PAD
    0x000170c8   0x000170c8   0x00000010   Code   RO         1660    i.drv_timer_get_instance  CVWL568.lib(drv_timer.o)
    0x000170d8   0x000170d8   0x0000000e   Code   RO         1662    i.drv_timer_get_prescaler  CVWL568.lib(drv_timer.o)
    0x000170e6   0x000170e6   0x00000002   PAD
    0x000170e8   0x000170e8   0x00000044   Code   RO         1663    i.drv_timer_handle_interrupt  CVWL568.lib(drv_timer.o)
    0x0001712c   0x0001712c   0x00000014   Code   RO         1664    i.drv_timer_register_callback  CVWL568.lib(drv_timer.o)
    0x00017140   0x00017140   0x0000000c   Code   RO         1665    i.drv_timer_set_current_count  CVWL568.lib(drv_timer.o)
    0x0001714c   0x0001714c   0x00000048   Code   RO         1666    i.drv_timer_set_int  CVWL568.lib(drv_timer.o)
    0x00017194   0x00017194   0x0000000c   Code   RO         1667    i.drv_timer_set_match  CVWL568.lib(drv_timer.o)
    0x000171a0   0x000171a0   0x00000016   Code   RO         1668    i.drv_timer_set_prescaler  CVWL568.lib(drv_timer.o)
    0x000171b6   0x000171b6   0x0000000a   Code   RO         1883    i.drv_tx_phy_test_clear  CVWL568.lib(drv_dsi_tx.o)
    0x000171c0   0x000171c0   0x0000001c   Code   RO         1884    i.drv_tx_phy_test_enter  CVWL568.lib(drv_dsi_tx.o)
    0x000171dc   0x000171dc   0x0000001c   Code   RO         1885    i.drv_tx_phy_test_exit  CVWL568.lib(drv_dsi_tx.o)
    0x000171f8   0x000171f8   0x00000012   Code   RO         1887    i.drv_tx_phy_test_write_1_byte  CVWL568.lib(drv_dsi_tx.o)
    0x0001720a   0x0001720a   0x00000014   Code   RO         1888    i.drv_tx_phy_test_write_2_byte  CVWL568.lib(drv_dsi_tx.o)
    0x0001721e   0x0001721e   0x00000010   Code   RO         1889    i.drv_tx_phy_test_write_code  CVWL568.lib(drv_dsi_tx.o)
    0x0001722e   0x0001722e   0x00000008   Code   RO         2131    i.drv_vidc_clear_irq  CVWL568.lib(drv_vidc.o)
    0x00017236   0x00017236   0x00000018   Code   RO         2135    i.drv_vidc_enable   CVWL568.lib(drv_vidc.o)
    0x0001724e   0x0001724e   0x00000002   PAD
    0x00017250   0x00017250   0x00000040   Code   RO         2136    i.drv_vidc_enable_irq  CVWL568.lib(drv_vidc.o)
    0x00017290   0x00017290   0x00000012   Code   RO         2138    i.drv_vidc_get_irq_status  CVWL568.lib(drv_vidc.o)
    0x000172a2   0x000172a2   0x00000002   PAD
    0x000172a4   0x000172a4   0x00000028   Code   RO         2142    i.drv_vidc_init_module_enable  CVWL568.lib(drv_vidc.o)
    0x000172cc   0x000172cc   0x0000000c   Code   RO         2143    i.drv_vidc_register_callback  CVWL568.lib(drv_vidc.o)
    0x000172d8   0x000172d8   0x00000006   Code   RO         2144    i.drv_vidc_reset    CVWL568.lib(drv_vidc.o)
    0x000172de   0x000172de   0x0000003c   Code   RO         2146    i.drv_vidc_set_dst_parameter  CVWL568.lib(drv_vidc.o)
    0x0001731a   0x0001731a   0x00000014   Code   RO         2150    i.drv_vidc_set_irqen  CVWL568.lib(drv_vidc.o)
    0x0001732e   0x0001732e   0x00000010   Code   RO         2151    i.drv_vidc_set_mirror  CVWL568.lib(drv_vidc.o)
    0x0001733e   0x0001733e   0x00000008   Code   RO         2154    i.drv_vidc_set_p2r_hcoef0  CVWL568.lib(drv_vidc.o)
    0x00017346   0x00017346   0x00000026   Code   RO         2155    i.drv_vidc_set_p2r_hinitb  CVWL568.lib(drv_vidc.o)
    0x0001736c   0x0001736c   0x00000026   Code   RO         2156    i.drv_vidc_set_p2r_hinitr  CVWL568.lib(drv_vidc.o)
    0x00017392   0x00017392   0x00000002   PAD
    0x00017394   0x00017394   0x00000018   Code   RO         2157    i.drv_vidc_set_pentile_swap  CVWL568.lib(drv_vidc.o)
    0x000173ac   0x000173ac   0x0000000a   Code   RO         2158    i.drv_vidc_set_pu_ctrl  CVWL568.lib(drv_vidc.o)
    0x000173b6   0x000173b6   0x00000010   Code   RO         2159    i.drv_vidc_set_rotation  CVWL568.lib(drv_vidc.o)
    0x000173c6   0x000173c6   0x0000000a   Code   RO         2160    i.drv_vidc_set_scld_hcoef0  CVWL568.lib(drv_vidc.o)
    0x000173d0   0x000173d0   0x0000000a   Code   RO         2161    i.drv_vidc_set_scld_hcoef1  CVWL568.lib(drv_vidc.o)
    0x000173da   0x000173da   0x00000012   Code   RO         2162    i.drv_vidc_set_scld_step  CVWL568.lib(drv_vidc.o)
    0x000173ec   0x000173ec   0x0000000a   Code   RO         2163    i.drv_vidc_set_scld_vcoef0  CVWL568.lib(drv_vidc.o)
    0x000173f6   0x000173f6   0x0000000a   Code   RO         2164    i.drv_vidc_set_scld_vcoef1  CVWL568.lib(drv_vidc.o)
    0x00017400   0x00017400   0x00000016   Code   RO         2165    i.drv_vidc_set_src_parameter  CVWL568.lib(drv_vidc.o)
    0x00017416   0x00017416   0x00000002   PAD
    0x00017418   0x00017418   0x00000010   Code   RO         2577    i.drv_wdg_clear_counter  CVWL568.lib(drv_wdg.o)
    0x00017428   0x00017428   0x00000010   Code   RO         2578    i.drv_wdg_clear_edge_flag  CVWL568.lib(drv_wdg.o)
    0x00017438   0x00017438   0x00000010   Code   RO         2581    i.drv_wdg_read_edge_flag  CVWL568.lib(drv_wdg.o)
    0x00017448   0x00017448   0x00000034   Code   RO         2584    i.drv_wdg_set_int   CVWL568.lib(drv_wdg.o)
    0x0001747c   0x0001747c   0x0000000a   Code   RO         1305    i.fls_clr_interrupt_flag  CVWL568.lib(drv_fls.o)
    0x00017486   0x00017486   0x00000014   Code   RO          892    i.fputc             CVWL568.lib(tau_log.o)
    0x0001749a   0x0001749a   0x00000002   PAD
    0x0001749c   0x0001749c   0x00000030   Code   RO          535    i.hal_dsi_rx_ctrl_create_handle  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000174cc   0x000174cc   0x0000009c   Code   RO          537    i.hal_dsi_rx_ctrl_deinit  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017568   0x00017568   0x00000084   Code   RO          539    i.hal_dsi_rx_ctrl_dsc_async_handler  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000175ec   0x000175ec   0x00000028   Code   RO          541    i.hal_dsi_rx_ctrl_gen_a_tear_signal  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017614   0x00017614   0x00000028   Code   RO          543    i.hal_dsi_rx_ctrl_get_max_ret_size  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001763c   0x0001763c   0x00000098   Code   RO          545    i.hal_dsi_rx_ctrl_init  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000176d4   0x000176d4   0x00000130   Code   RO          546    i.hal_dsi_rx_ctrl_init_clk  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017804   0x00017804   0x000000d4   Code   RO          547    i.hal_dsi_rx_ctrl_init_dsi_rx  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000178d8   0x000178d8   0x0000013c   Code   RO          548    i.hal_dsi_rx_ctrl_init_memc  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017a14   0x00017a14   0x00000130   Code   RO          549    i.hal_dsi_rx_ctrl_init_rxbr  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017b44   0x00017b44   0x0000022c   Code   RO          550    i.hal_dsi_rx_ctrl_init_vidc  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017d70   0x00017d70   0x0000003c   Code   RO          551    i.hal_dsi_rx_ctrl_pre_init_pps  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017dac   0x00017dac   0x000000f0   Code   RO          554    i.hal_dsi_rx_ctrl_send_ack_cmd  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017e9c   0x00017e9c   0x0000002c   Code   RO          556    i.hal_dsi_rx_ctrl_set_cus_esc_clk  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017ec8   0x00017ec8   0x0000006c   Code   RO          557    i.hal_dsi_rx_ctrl_set_cus_scld_filter  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017f34   0x00017f34   0x00000034   Code   RO          558    i.hal_dsi_rx_ctrl_set_cus_sync_line  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017f68   0x00017f68   0x00000038   Code   RO          562    i.hal_dsi_rx_ctrl_set_ipi_cfg  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00017fa0   0x00017fa0   0x00000072   Code   RO          566    i.hal_dsi_rx_ctrl_set_rxbr_clk  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00018012   0x00018012   0x00000002   PAD
    0x00018014   0x00018014   0x00000034   Code   RO          567    i.hal_dsi_rx_ctrl_set_sw_tear_mode  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00018048   0x00018048   0x0000000e   Code   RO          569    i.hal_dsi_rx_ctrl_set_tear_mode_ex  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00018056   0x00018056   0x00000002   PAD
    0x00018058   0x00018058   0x0000003c   Code   RO          570    i.hal_dsi_rx_ctrl_start  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00018094   0x00018094   0x0000003c   Code   RO          571    i.hal_dsi_rx_ctrl_stop  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000180d0   0x000180d0   0x00000020   Code   RO          573    i.hal_dsi_rx_ctrl_toggle_resolution  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000180f0   0x000180f0   0x00000190   Code   RO          624    i.hal_dsi_tx_calc_video_chunks  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018280   0x00018280   0x00000034   Code   RO          625    i.hal_dsi_tx_config_params_for_lane_rate  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000182b4   0x000182b4   0x000004d0   Code   RO          626    i.hal_dsi_tx_count_lane_rate  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018784   0x00018784   0x0000002c   Code   RO          628    i.hal_dsi_tx_ctrl_create_handle  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000187b0   0x000187b0   0x00000048   Code   RO          629    i.hal_dsi_tx_ctrl_deinit  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000187f8   0x000187f8   0x0000004c   Code   RO          630    i.hal_dsi_tx_ctrl_enter_init_panel_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018844   0x00018844   0x00000028   Code   RO          632    i.hal_dsi_tx_ctrl_exit_init_panel_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001886c   0x0001886c   0x000000c4   Code   RO          634    i.hal_dsi_tx_ctrl_init  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018930   0x00018930   0x00000024   Code   RO          635    i.hal_dsi_tx_ctrl_init_clk  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018954   0x00018954   0x0000000c   Code   RO          636    i.hal_dsi_tx_ctrl_panel_reset_pin  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018960   0x00018960   0x00000020   Code   RO          639    i.hal_dsi_tx_ctrl_set_ccm  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018980   0x00018980   0x00000014   Code   RO          645    i.hal_dsi_tx_ctrl_set_overwrite_rgb  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018994   0x00018994   0x00000010   Code   RO          646    i.hal_dsi_tx_ctrl_set_partial_disp  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000189a4   0x000189a4   0x00000024   Code   RO          647    i.hal_dsi_tx_ctrl_set_partial_disp_area  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000189c8   0x000189c8   0x0000006c   Code   RO          649    i.hal_dsi_tx_ctrl_start  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018a34   0x00018a34   0x00000044   Code   RO          650    i.hal_dsi_tx_ctrl_stop  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018a78   0x00018a78   0x000000d8   Code   RO          651    i.hal_dsi_tx_ctrl_write_array_cmd  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018b50   0x00018b50   0x000000b0   Code   RO          652    i.hal_dsi_tx_ctrl_write_cmd  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018c00   0x00018c00   0x00000044   Code   RO          653    i.hal_dsi_tx_init_data_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018c44   0x00018c44   0x00000030   Code   RO          654    i.hal_dsi_tx_init_dpi_cfg  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018c74   0x00018c74   0x00000020   Code   RO          655    i.hal_dsi_tx_init_interrupt  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018c94   0x00018c94   0x00000020   Code   RO          656    i.hal_dsi_tx_init_phy_cfg  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018cb4   0x00018cb4   0x00000094   Code   RO          657    i.hal_dsi_tx_init_remains  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018d48   0x00018d48   0x00000058   Code   RO          658    i.hal_dsi_tx_init_video_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018da0   0x00018da0   0x00000044   Code   RO          659    i.hal_dsi_tx_send_cmd  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018de4   0x00018de4   0x00000018   Code   RO          717    i.hal_gpio_ctrl_eint  CVWL568.lib(hal_gpio.o)
    0x00018dfc   0x00018dfc   0x00000012   Code   RO          718    i.hal_gpio_get_input_data  CVWL568.lib(hal_gpio.o)
    0x00018e0e   0x00018e0e   0x00000002   PAD
    0x00018e10   0x00018e10   0x00000040   Code   RO          721    i.hal_gpio_init_eint  CVWL568.lib(hal_gpio.o)
    0x00018e50   0x00018e50   0x00000020   Code   RO          722    i.hal_gpio_init_input  CVWL568.lib(hal_gpio.o)
    0x00018e70   0x00018e70   0x00000028   Code   RO          723    i.hal_gpio_init_output  CVWL568.lib(hal_gpio.o)
    0x00018e98   0x00018e98   0x00000018   Code   RO          724    i.hal_gpio_reg_eint_cb  CVWL568.lib(hal_gpio.o)
    0x00018eb0   0x00018eb0   0x00000050   Code   RO          725    i.hal_gpio_set_ap_reset_int  CVWL568.lib(hal_gpio.o)
    0x00018f00   0x00018f00   0x00000060   Code   RO          727    i.hal_gpio_set_mode  CVWL568.lib(hal_gpio.o)
    0x00018f60   0x00018f60   0x00000008   Code   RO          728    i.hal_gpio_set_output_data  CVWL568.lib(hal_gpio.o)
    0x00018f68   0x00018f68   0x00000020   Code   RO          730    i.hal_gpio_set_pull_state  CVWL568.lib(hal_gpio.o)
    0x00018f88   0x00018f88   0x0000006c   Code   RO          755    i.hal_i2c_m_dma_init  CVWL568.lib(hal_i2c_master.o)
    0x00018ff4   0x00018ff4   0x00000020   Code   RO          756    i.hal_i2c_m_dma_read  CVWL568.lib(hal_i2c_master.o)
    0x00019014   0x00019014   0x0000001c   Code   RO          757    i.hal_i2c_m_dma_write  CVWL568.lib(hal_i2c_master.o)
    0x00019030   0x00019030   0x0000000c   Code   RO          759    i.hal_i2c_m_transfer_complate  CVWL568.lib(hal_i2c_master.o)
    0x0001903c   0x0001903c   0x00000020   Code   RO          760    i.hal_i2c_master_irq_callback  CVWL568.lib(hal_i2c_master.o)
    0x0001905c   0x0001905c   0x00000010   Code   RO          772    i.hal_i2c_s_dma_user_callback  CVWL568.lib(hal_i2c_slave.o)
    0x0001906c   0x0001906c   0x00000038   Code   RO          773    i.hal_i2c_s_dma_write  CVWL568.lib(hal_i2c_slave.o)
    0x000190a4   0x000190a4   0x0000006c   Code   RO          775    i.hal_i2c_s_init    CVWL568.lib(hal_i2c_slave.o)
    0x00019110   0x00019110   0x00000014   Code   RO          776    i.hal_i2c_s_nonblocking_read  CVWL568.lib(hal_i2c_slave.o)
    0x00019124   0x00019124   0x0000000c   Code   RO          783    i.hal_i2c_s_set_transfer  CVWL568.lib(hal_i2c_slave.o)
    0x00019130   0x00019130   0x0000014c   Code   RO          786    i.hal_i2c_slave_irq_callback  CVWL568.lib(hal_i2c_slave.o)
    0x0001927c   0x0001927c   0x000000e4   Code   RO         1701    i.hal_internal_init_memc  CVWL568.lib(hal_internal_vsync.o)
    0x00019360   0x00019360   0x00000010   Code   RO         1702    i.hal_internal_sync_get_fb_setting  CVWL568.lib(hal_internal_vsync.o)
    0x00019370   0x00019370   0x00000214   Code   RO         1703    i.hal_internal_sync_input_resolution_change  CVWL568.lib(hal_internal_vsync.o)
    0x00019584   0x00019584   0x0000001c   Code   RO         1705    i.hal_internal_vsync_deinit  CVWL568.lib(hal_internal_vsync.o)
    0x000195a0   0x000195a0   0x0000000c   Code   RO         1706    i.hal_internal_vsync_get_rx_state  CVWL568.lib(hal_internal_vsync.o)
    0x000195ac   0x000195ac   0x00000018   Code   RO         1707    i.hal_internal_vsync_get_sync_line  CVWL568.lib(hal_internal_vsync.o)
    0x000195c4   0x000195c4   0x0000000c   Code   RO         1708    i.hal_internal_vsync_get_tx_state  CVWL568.lib(hal_internal_vsync.o)
    0x000195d0   0x000195d0   0x000000fc   Code   RO         1709    i.hal_internal_vsync_init_rx  CVWL568.lib(hal_internal_vsync.o)
    0x000196cc   0x000196cc   0x000000b0   Code   RO         1710    i.hal_internal_vsync_init_tx  CVWL568.lib(hal_internal_vsync.o)
    0x0001977c   0x0001977c   0x0000011c   Code   RO         1711    i.hal_internal_vsync_set_auto_hw_filter  CVWL568.lib(hal_internal_vsync.o)
    0x00019898   0x00019898   0x00000014   Code   RO         1713    i.hal_internal_vsync_set_rx_state  CVWL568.lib(hal_internal_vsync.o)
    0x000198ac   0x000198ac   0x0000001c   Code   RO         1714    i.hal_internal_vsync_set_sync_line  CVWL568.lib(hal_internal_vsync.o)
    0x000198c8   0x000198c8   0x00000048   Code   RO         1715    i.hal_internal_vsync_set_tear_mode  CVWL568.lib(hal_internal_vsync.o)
    0x00019910   0x00019910   0x00000040   Code   RO         1716    i.hal_internal_vsync_set_tx_state  CVWL568.lib(hal_internal_vsync.o)
    0x00019950   0x00019950   0x00000024   Code   RO          660    i.hal_lcdc_config_ccm  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00019974   0x00019974   0x00000048   Code   RO          661    i.hal_lcdc_config_remains  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000199bc   0x000199bc   0x00000014   Code   RO          662    i.hal_lcdc_config_rgb_to_pentile  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000199d0   0x000199d0   0x00000164   Code   RO          663    i.hal_lcdc_config_upscaler  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00019b34   0x00019b34   0x00000040   Code   RO          664    i.hal_lcdc_init_cfg  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00019b74   0x00019b74   0x00000180   Code   RO          665    i.hal_lcdc_init_clk  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00019cf4   0x00019cf4   0x00000040   Code   RO          666    i.hal_lcdc_init_interrupt  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00019d34   0x00019d34   0x0000000e   Code   RO          808    i.hal_spi_m_clear_rxfifo  CVWL568.lib(hal_spi_master.o)
    0x00019d42   0x00019d42   0x00000008   Code   RO          832    i.hal_system_enable_systick  CVWL568.lib(hal_system.o)
    0x00019d4a   0x00019d4a   0x00000002   PAD
    0x00019d4c   0x00019d4c   0x00000088   Code   RO          837    i.hal_system_init   CVWL568.lib(hal_system.o)
    0x00019dd4   0x00019dd4   0x0000001c   Code   RO          838    i.hal_system_init_console  CVWL568.lib(hal_system.o)
    0x00019df0   0x00019df0   0x00000008   Code   RO          841    i.hal_system_set_phy_calibration  CVWL568.lib(hal_system.o)
    0x00019df8   0x00019df8   0x00000008   Code   RO          842    i.hal_system_set_pvd  CVWL568.lib(hal_system.o)
    0x00019e00   0x00019e00   0x00000008   Code   RO          843    i.hal_system_set_vcc  CVWL568.lib(hal_system.o)
    0x00019e08   0x00019e08   0x0000001a   Code   RO          868    i.hal_timer_init    CVWL568.lib(hal_timer.o)
    0x00019e22   0x00019e22   0x00000002   PAD
    0x00019e24   0x00019e24   0x00000050   Code   RO          870    i.hal_timer_start   CVWL568.lib(hal_timer.o)
    0x00019e74   0x00019e74   0x0000008c   Code   RO         1033    i.hal_uart_init     CVWL568.lib(hal_uart.o)
    0x00019f00   0x00019f00   0x00000010   Code   RO         1036    i.hal_uart_transmit_blocking  CVWL568.lib(hal_uart.o)
    0x00019f10   0x00019f10   0x00000110   Code   RO         2241    i.handle_init       CVWL568.lib(irq_redirect .o)
    0x0001a020   0x0001a020   0x00000070   Code   RO          111    i.init_mipi_tx      ap_demo.o
    0x0001a090   0x0001a090   0x00000098   Code   RO          112    i.init_panel        ap_demo.o
    0x0001a128   0x0001a128   0x0000000a   Code   RO            3    i.main              main.o
    0x0001a132   0x0001a132   0x00000002   PAD
    0x0001a134   0x0001a134   0x000000c8   Code   RO          113    i.open_mipi_rx      ap_demo.o
    0x0001a1fc   0x0001a1fc   0x000000c0   Code   RO          114    i.pps_update_handle  ap_demo.o
    0x0001a2bc   0x0001a2bc   0x000003f4   Code   RO         1717    i.rx_get_dcs_packet_data  CVWL568.lib(hal_internal_vsync.o)
    0x0001a6b0   0x0001a6b0   0x00000140   Code   RO         1718    i.rx_partial_update  CVWL568.lib(hal_internal_vsync.o)
    0x0001a7f0   0x0001a7f0   0x0000008c   Code   RO         1719    i.rx_receive_packet  CVWL568.lib(hal_internal_vsync.o)
    0x0001a87c   0x0001a87c   0x00000180   Code   RO         1720    i.rx_receive_pps    CVWL568.lib(hal_internal_vsync.o)
    0x0001a9fc   0x0001a9fc   0x000000a4   Code   RO         1721    i.rxbr_irq0_callback  CVWL568.lib(hal_internal_vsync.o)
    0x0001aaa0   0x0001aaa0   0x00000170   Code   RO         1722    i.rxbr_irq1_callback  CVWL568.lib(hal_internal_vsync.o)
    0x0001ac10   0x0001ac10   0x0000008c   Code   RO         1723    i.soft_gen_te       CVWL568.lib(hal_internal_vsync.o)
    0x0001ac9c   0x0001ac9c   0x00000030   Code   RO          115    i.soft_timer3_cb    ap_demo.o
    0x0001accc   0x0001accc   0x00000048   Code   RO         2626    i.sqrt              m_ps.l(sqrt.o)
    0x0001ad14   0x0001ad14   0x00000068   Code   RO          116    i.tp_heartbeat_exec  ap_demo.o
    0x0001ad7c   0x0001ad7c   0x000000e8   Code   RO         1724    i.vidc_callback     CVWL568.lib(hal_internal_vsync.o)
    0x0001ae64   0x0001ae64   0x000000d0   Code   RO         1725    i.vpre_err_reset    CVWL568.lib(hal_internal_vsync.o)
    0x0001af34   0x0001af34   0x0000019c   Code   RO         1726    i.vsync_set_te_mode  CVWL568.lib(hal_internal_vsync.o)
    0x0001b0d0   0x0001b0d0   0x000024b8   Data   RO          117    .constdata          ap_demo.o
    0x0001d588   0x0001d588   0x00000020   Data   RO          418    .constdata          app_tp_st_touch.o
    0x0001d5a8   0x0001d5a8   0x000000d2   Data   RO          733    .constdata          CVWL568.lib(hal_gpio.o)
    0x0001d67a   0x0001d67a   0x000014a6   Data   RO          904    .constdata          WL568_S21_NT37701_TP.lib(app_tp_for_custom_s8.o)
    0x0001eb20   0x0001eb20   0x00000001   Data   RO          919    .constdata          WL568_S21_NT37701_TP.lib(app_tp_for_custom_s8.o)
    0x0001eb21   0x0001eb21   0x00000003   PAD
    0x0001eb24   0x0001eb24   0x00000008   Data   RO         1536    .constdata          CVWL568.lib(drv_param_init.o)
    0x0001eb2c   0x0001eb2c   0x00000186   Data   RO         2291    .constdata          CVWL568.lib(drv_phy_common.o)
    0x0001ecb2   0x0001ecb2   0x00000002   PAD
    0x0001ecb4   0x0001ecb4   0x00000048   Data   RO          575    .conststring        CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001ecfc   0x0001ecfc   0x00000134   Data   RO         1728    .conststring        CVWL568.lib(hal_internal_vsync.o)
    0x0001ee30   0x0001ee30   0x00000030   Data   RO         2988    Region$$Table       anon$$obj.o


    Execution Region RW_RAM1 (Exec base: 0x00070000, Load base: 0x0001ee60, Size: 0x00000000, Max: 0x000000f0, ABSOLUTE)

    **** No section assigned to this execution region ****


    Execution Region RW_RAM2 (Exec base: 0x00070100, Load base: 0x0001ee60, Size: 0x000000c0, Max: 0x000000d0, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00070100        -       0x000000c0   Zero   RW         2242    .ARM.__AT_0x00070100  CVWL568.lib(irq_redirect .o)


    Execution Region RW_RAM3 (Exec base: 0x000701d0, Load base: 0x0001ee60, Size: 0x000038f0, Max: 0x00007e30, ABSOLUTE, COMPRESSED[0x00000554])

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x000701d0   COMPRESSED   0x0000022c   Data   RW          118    .data               ap_demo.o
    0x000703fc   COMPRESSED   0x00000017   Data   RW          270    .data               app_tp_transfer.o
    0x00070413   COMPRESSED   0x00000028   Data   RW          419    .data               app_tp_st_touch.o
    0x0007043b   COMPRESSED   0x00000001   PAD
    0x0007043c   COMPRESSED   0x00000008   Data   RW          576    .data               CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00070444   COMPRESSED   0x00000001   Data   RW          668    .data               CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00070445   COMPRESSED   0x00000001   Data   RW          761    .data               CVWL568.lib(hal_i2c_master.o)
    0x00070446   COMPRESSED   0x00000002   PAD
    0x00070448   COMPRESSED   0x0000001c   Data   RW          787    .data               CVWL568.lib(hal_i2c_slave.o)
    0x00070464   COMPRESSED   0x000000e4   Data   RW          920    .data               WL568_S21_NT37701_TP.lib(app_tp_for_custom_s8.o)
    0x00070548   COMPRESSED   0x00000001   Data   RW          921    .data               WL568_S21_NT37701_TP.lib(app_tp_for_custom_s8.o)
    0x00070549   COMPRESSED   0x00000001   Data   RW          922    .data               WL568_S21_NT37701_TP.lib(app_tp_for_custom_s8.o)
    0x0007054a   COMPRESSED   0x00000001   Data   RW          927    .data               WL568_S21_NT37701_TP.lib(app_tp_for_custom_s8.o)
    0x0007054b   COMPRESSED   0x00000003   Data   RW          928    .data               WL568_S21_NT37701_TP.lib(app_tp_for_custom_s8.o)
    0x0007054e   COMPRESSED   0x00000005   Data   RW          929    .data               WL568_S21_NT37701_TP.lib(app_tp_for_custom_s8.o)
    0x00070553   COMPRESSED   0x00000001   PAD
    0x00070554   COMPRESSED   0x00000030   Data   RW          939    .data               WL568_S21_NT37701_TP.lib(app_tp_for_custom_s8.o)
    0x00070584   COMPRESSED   0x00000012   Data   RW         1090    .data               CVWL568.lib(norflash.o)
    0x00070596   COMPRESSED   0x00000002   PAD
    0x00070598   COMPRESSED   0x0000000c   Data   RW         1143    .data               CVWL568.lib(drv_common.o)
    0x000705a4   COMPRESSED   0x00000004   Data   RW         1408    .data               CVWL568.lib(drv_gpio.o)
    0x000705a8   COMPRESSED   0x00000008   Data   RW         1446    .data               CVWL568.lib(drv_i2c_dma.o)
    0x000705b0   COMPRESSED   0x00000004   Data   RW         1474    .data               CVWL568.lib(drv_i2c_master.o)
    0x000705b4   COMPRESSED   0x00000008   Data   RW         1508    .data               CVWL568.lib(drv_i2c_slave.o)
    0x000705bc   COMPRESSED   0x000004a4   Data   RW         1537    .data               CVWL568.lib(drv_param_init.o)
    0x00070a60   COMPRESSED   0x00000004   Data   RW         1602    .data               CVWL568.lib(drv_spi_master.o)
    0x00070a64   COMPRESSED   0x00000001   Data   RW         1634    .data               CVWL568.lib(drv_sys_cfg.o)
    0x00070a65   COMPRESSED   0x00000003   PAD
    0x00070a68   COMPRESSED   0x00000050   Data   RW         1670    .data               CVWL568.lib(drv_timer.o)
    0x00070ab8   COMPRESSED   0x00000004   Data   RW         1729    .data               CVWL568.lib(hal_internal_vsync.o)
    0x00070abc   COMPRESSED   0x00000008   Data   RW         2094    .data               CVWL568.lib(drv_rxbr.o)
    0x00070ac4   COMPRESSED   0x00000004   Data   RW         2167    .data               CVWL568.lib(drv_vidc.o)
    0x00070ac8   COMPRESSED   0x00000001   Data   RW         2292    .data               CVWL568.lib(drv_phy_common.o)
    0x00070ac9   COMPRESSED   0x00000003   PAD
    0x00070acc   COMPRESSED   0x0000000c   Data   RW         2312    .data               CVWL568.lib(drv_chip_info.o)
    0x00070ad8   COMPRESSED   0x0000000c   Data   RW         2422    .data               CVWL568.lib(drv_pwm.o)
    0x00070ae4   COMPRESSED   0x00000008   Data   RW         2477    .data               CVWL568.lib(drv_swire.o)
    0x00070aec   COMPRESSED   0x00000008   Data   RW         2519    .data               CVWL568.lib(drv_uart.o)
    0x00070af4   COMPRESSED   0x0000000c   Data   RW         2586    .data               CVWL568.lib(drv_wdg.o)
    0x00070b00   COMPRESSED   0x00000004   Data   RW         2957    .data               mc_p.l(stdout.o)
    0x00070b04   COMPRESSED   0x00000004   Data   RW         2969    .data               mc_p.l(errno.o)
    0x00070b08        -       0x00000190   Zero   RW          269    .bss                app_tp_transfer.o
    0x00070c98        -       0x0000000c   Zero   RW          417    .bss                app_tp_st_touch.o
    0x00070ca4        -       0x000000c0   Zero   RW          574    .bss                CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00070d64        -       0x00000048   Zero   RW          667    .bss                CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00070dac        -       0x00000100   Zero   RW          893    .bss                CVWL568.lib(tau_log.o)
    0x00070eac        -       0x000000d0   Zero   RW         1038    .bss                CVWL568.lib(hal_uart.o)
    0x00070f7c        -       0x0000001c   Zero   RW         1270    .bss                CVWL568.lib(drv_dma.o)
    0x00070f98        -       0x00000040   Zero   RW         1407    .bss                CVWL568.lib(drv_gpio.o)
    0x00070fd8        -       0x00000140   Zero   RW         1445    .bss                CVWL568.lib(drv_i2c_dma.o)
    0x00071118        -       0x00000958   Zero   RW         1727    .bss                CVWL568.lib(hal_internal_vsync.o)
    0x00071a70        -       0x00001030   Zero   RW         1771    .bss                CVWL568.lib(dcs_packet_fifo.o)
    0x00072aa0        -       0x00000020   Zero   RW         2356    .bss                CVWL568.lib(hal_spi_slave.o)
    0x00072ac0        -       0x00001000   Zero   RW          524    STACK               startup_armcm0.o


==============================================================================

Image component sizes


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Object Name

      6122        818       9400        556          0      38729   ap_demo.o
      1298        244         32         40         12      12693   app_tp_st_touch.o
      1004        148          0         23        400      14112   app_tp_transfer.o
        36          6          0          0          0        573   board.o
        10          0          0          0          0       5723   main.o
       120         18        192          0       4096       2124   startup_armcm0.o

    ----------------------------------------------------------------------
      8596       1234       9672        620       4508      73954   Object Totals
         0          0         48          0          0          0   (incl. Generated)
         6          0          0          1          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Member Name

       216         32          0          0       4144        252   dcs_packet_fifo.o
       296         96          0         12          0        256   drv_chip_info.o
       192         82         20         12          0        264   drv_common.o
       420         90          0          0          0       1200   drv_crgu.o
       410         28          0          0         28        796   drv_dma.o
       232         28          0          0          0        340   drv_dsc_dec.o
      1624        494          0          0          0       1332   drv_dsi_rx.o
      1476        118          0          0          0       2428   drv_dsi_tx.o
       118          0          0          0          0        256   drv_efuse.o
        10          0          0          0          0         60   drv_fls.o
       784        112          0          4         64       1236   drv_gpio.o
       588         88          0          8        320        624   drv_i2c_dma.o
       360         86          0          4          0        456   drv_i2c_master.o
       324         74          0          8          0        516   drv_i2c_slave.o
       668          6          0          0          0       1444   drv_lcdc.o
       492         28          0          0          0       1112   drv_memc.o
       212         44          8       1188          0        452   drv_param_init.o
       428         30        390          1          0        664   drv_phy_common.o
        72         10          0         12          0         76   drv_pwm.o
       104         24          0          0          0        180   drv_pwr.o
       682         66          0          8          0       1448   drv_rxbr.o
       104         24          0          4          0        188   drv_spi_master.o
       104         12          0          8          0        140   drv_swire.o
       300         64          0          1          0        628   drv_sys_cfg.o
       334         22          0         80          0        944   drv_timer.o
       698         18          0          8          0        680   drv_uart.o
       510         28          0          4          0       1452   drv_vidc.o
       156         22          0         12          0        316   drv_wdg.o
      3178        308         72          8        192       1760   hal_dsi_rx_ctrl.o
      4312        278          0          1         72       2384   hal_dsi_tx_ctrl.o
       450         48        210          0          0        752   hal_gpio.o
       212         40          0          1          0        340   hal_i2c_master.o
       544         76          0         28          0        400   hal_i2c_slave.o
      6580       1504        308          4       2392       2264   hal_internal_vsync.o
        14          0          0          0          0         68   hal_spi_master.o
       580         32          0          0         32        136   hal_spi_slave.o
       196         32          0          0          0        408   hal_system.o
       106          6          0          0          0        140   hal_timer.o
       156         18          0          0        208        144   hal_uart.o
      1076        324          0          0        192       1980   irq_redirect .o
        48         10          0         18          0         68   norflash.o
        58          0          0          0          0        128   tau_delay.o
        60         10          0          0        256        156   tau_log.o
      1536         60       5287        287          0      17772   app_tp_for_custom_s8.o
       200         20          0          0          0         76   ceil.o
        72          6          0          0          0         76   sqrt.o
        86          0          0          0          0          0   __dczerorl2.o
         0          0          0          0          0          0   entry.o
         0          0          0          0          0          0   entry10a.o
         0          0          0          0          0          0   entry11a.o
         8          4          0          0          0          0   entry2.o
         4          0          0          0          0          0   entry5.o
         0          0          0          0          0          0   entry7b.o
         0          0          0          0          0          0   entry8b.o
         8          4          0          0          0          0   entry9a.o
        12          6          0          4          0         60   errno.o
        30          0          0          0          0          0   handlers.o
        40          0          0          0          0         72   idiv.o
        36          8          0          0          0         68   init.o
         0          0          0          0          0          0   iusefp.o
        32          0          0          0          0         68   llshl.o
        38          0          0          0          0         68   llsshr.o
        34          0          0          0          0         68   llushr.o
        36          0          0          0          0         60   memcpya.o
        36          0          0          0          0        100   memseta.o
      2298        104          0          0          0        544   printfa.o
         0          0          0          4          0          0   stdout.o
        44          0          0          0          0         72   uidiv.o
        96          0          0          0          0         84   uldiv.o
        40          2          0          0          0         68   cdcmple.o
        40          2          0          0          0         68   cdrcmple.o
        20          0          0          0          0         68   cfrcmple.o
       356          4          0          0          0        140   dadd.o
       240          6          0          0          0         84   ddiv.o
       236          0          0          0          0        216   depilogue.o
        72         10          0          0          0         72   dfixi.o
        60         10          0          0          0         68   dfixui.o
        64         10          0          0          0         68   dfixul.o
        28          4          0          0          0         68   dfltui.o
       208          6          0          0          0         88   dmul.o
       162          0          0          0          0         80   dsqrt.o
        40          0          0          0          0         60   f2d.o
       178          0          0          0          0        108   fadd.o
       124          0          0          0          0         72   fdiv.o
       130          0          0          0          0        144   fepilogue.o
        50          0          0          0          0         60   ffixi.o
        40          0          0          0          0         60   ffixui.o
        22          0          0          0          0         68   fflti.o
        14          0          0          0          0         68   ffltui.o
       122          0          0          0          0         72   fmul.o
        24          0          0          0          0         60   fscalb.o

    ----------------------------------------------------------------------
     36456       4678       6300       1740       7900      51916   Library Totals
        56          0          5         11          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Name

     29484       4412       1008       1434       7900      30868   CVWL568.lib
      1536         60       5287        287          0      17772   WL568_S21_NT37701_TP.lib
       272         26          0          0          0        152   m_ps.l
      2838        126          0          8          0       1264   mc_p.l
      2270         54          0          0          0       1860   mf_p.l

    ----------------------------------------------------------------------
     36456       4678       6300       1740       7900      51916   Library Totals

    ----------------------------------------------------------------------

==============================================================================


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   

     45052       5912      15972       2360      12408     101870   Grand Totals
     45052       5912      15972       1364      12408     101870   ELF Image Totals (compressed)
     45052       5912      15972       1364          0          0   ROM Totals

==============================================================================

    Total RO  Size (Code + RO Data)                61024 (  59.59kB)
    Total RW  Size (RW Data + ZI Data)             14768 (  14.42kB)
    Total ROM Size (Code + RO Data + RW Data)      62388 (  60.93kB)

==============================================================================

