Component: ARM Compiler 5.06 update 6 (build 750) Tool: armlink [4d35ed]

==============================================================================

Section Cross References

    main.o(i.main) refers to board.o(i.board_Init) for board_Init
    main.o(i.main) refers to ap_demo.o(i.ap_demo) for ap_demo
    ap_demo.o(i.Gpio_swire_output) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    ap_demo.o(i.Gpio_swire_output) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.Gpio_swire_output) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    ap_demo.o(i.Gpio_swire_output) refers to tau_delay.o(i.delayUs) for delayUs
    ap_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) for hal_dsi_rx_ctrl_get_max_ret_size
    ap_demo.o(i.ap_dcs_read) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) for hal_dsi_rx_ctrl_send_ack_cmd
    ap_demo.o(i.ap_dcs_read) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_dcs_read) refers to app_tp_st_touch.o(i.ap_get_tp_calibration_status_01) for ap_get_tp_calibration_status_01
    ap_demo.o(i.ap_demo) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.open_mipi_rx) for open_mipi_rx
    ap_demo.o(i.ap_demo) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.init_mipi_tx) for init_mipi_tx
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.init_panel) for init_panel
    ap_demo.o(i.ap_demo) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    ap_demo.o(i.ap_demo) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.ap_demo) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_demo) refers to memcpya.o(.text) for __aeabi_memcpy4
    ap_demo.o(i.ap_demo) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) for hal_dsi_tx_ctrl_set_ccm
    ap_demo.o(i.ap_demo) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) for hal_dsi_rx_ctrl_dsc_async_handler
    ap_demo.o(i.ap_demo) refers to app_tp_for_custom_s8.o(.data) for tp_sleep_in
    ap_demo.o(i.ap_demo) refers to ap_demo.o(.bss) for .bss
    ap_demo.o(i.ap_demo) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_get_reg_df) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_get_reg_df) refers to ap_demo.o(.bss) for .bss
    ap_demo.o(i.ap_set_backlight_51) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_backlight_51) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_backlight_51) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_set_display_off) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_display_off) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_display_on) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to ap_demo.o(i.Gpio_swire_output) for Gpio_swire_output
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin) for hal_dsi_tx_ctrl_panel_reset_pin
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_set_exit_sleep_mode) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_exit_sleep_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_exit_sleep_mode) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.ap_set_exit_sleep_mode) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) for hal_dsi_rx_ctrl_toggle_resolution
    ap_demo.o(i.ap_set_exit_sleep_mode) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_set_hbm_53) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_hbm_53) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_update_frame_rate) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex) for hal_dsi_rx_ctrl_set_tear_mode_ex
    ap_demo.o(i.ap_update_frame_rate) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.frame_start_cb) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) for hal_dsi_rx_ctrl_restart
    ap_demo.o(i.frame_start_cb) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.frame_start_cb) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.init_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) for hal_dsi_tx_ctrl_create_handle
    ap_demo.o(i.init_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    ap_demo.o(i.init_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) for hal_dsi_tx_ctrl_set_overwrite_rgb
    ap_demo.o(i.init_mipi_tx) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin) for hal_dsi_tx_ctrl_panel_reset_pin
    ap_demo.o(i.init_panel) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) for hal_dsi_tx_ctrl_enter_init_panel_mode
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) for hal_dsi_tx_ctrl_write_array_cmd
    ap_demo.o(i.init_panel) refers to tau_delay.o(i.delayUs) for delayUs
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.init_panel) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    ap_demo.o(i.init_panel) refers to ap_demo.o(i.Gpio_swire_output) for Gpio_swire_output
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) for hal_dsi_tx_ctrl_exit_init_panel_mode
    ap_demo.o(i.init_panel) refers to ap_demo.o(.constdata) for .constdata
    ap_demo.o(i.open_mipi_rx) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) for hal_dsi_rx_ctrl_create_handle
    ap_demo.o(i.open_mipi_rx) refers to memcpya.o(.text) for __aeabi_memcpy4
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) for hal_dsi_rx_ctrl_pre_init_pps
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) for hal_dsi_rx_ctrl_set_cus_sync_line
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) for hal_dsi_rx_ctrl_set_cus_scld_filter
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) for hal_dsi_rx_ctrl_set_cus_esc_clk
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(.constdata) for .constdata
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(i.ap_dcs_read) for ap_dcs_read
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(i.pps_update_handle) for pps_update_handle
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(i.frame_start_cb) for frame_start_cb
    ap_demo.o(i.pps_update_handle) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) for hal_dsi_rx_ctrl_toggle_resolution
    ap_demo.o(i.pps_update_handle) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.pps_update_handle) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.tp_heartbeat_exec) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    ap_demo.o(i.tp_heartbeat_exec) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.tp_heartbeat_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) for ap_tp_st_touch_hardware_reset
    ap_demo.o(i.tp_heartbeat_exec) refers to app_tp_transfer.o(.data) for s_screen_init_complate
    ap_demo.o(i.tp_heartbeat_exec) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.tp_power_up_restart) refers to app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) for ap_tp_st_touch_hardware_reset
    ap_demo.o(i.tp_power_up_restart) refers to ap_demo.o(.data) for .data
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_display_on) for ap_set_display_on
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_display_off) for ap_set_display_off
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_get_reg_df) for ap_get_reg_df
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_backlight_51) for ap_set_backlight_51
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_update_frame_rate) for ap_update_frame_rate
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_hbm_53) for ap_set_hbm_53
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_enter_sleep_mode) for ap_set_enter_sleep_mode
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_exit_sleep_mode) for ap_set_exit_sleep_mode
    app_tp_transfer.o(i.S20_Start_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_transfer.o(i.S20_Start_init) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.S20_Start_init) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_ctrl_eint) for hal_gpio_ctrl_eint
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_init_eint) for hal_gpio_init_eint
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_reg_eint_cb) for hal_gpio_reg_eint_cb
    app_tp_transfer.o(i.S20_Start_init) refers to ap_demo.o(.data) for s_power_up_flag
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_for_custom_s8.o(.data) for screen_reg_int_data
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(i.app_tp_screen_int_callback) for app_tp_screen_int_callback
    app_tp_transfer.o(i.S20_Start_init) refers to ap_demo.o(.data) for phone_start_flag
    app_tp_transfer.o(i.app_tp_I2C_init) refers to hal_i2c_slave.o(i.hal_i2c_s_init) for hal_i2c_s_init
    app_tp_transfer.o(i.app_tp_I2C_init) refers to hal_i2c_slave.o(i.hal_i2c_s_set_transfer) for hal_i2c_s_set_transfer
    app_tp_transfer.o(i.app_tp_I2C_init) refers to hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read) for hal_i2c_s_nonblocking_read
    app_tp_transfer.o(i.app_tp_I2C_init) refers to app_tp_transfer.o(i.app_tp_i2cs_callback) for app_tp_i2cs_callback
    app_tp_transfer.o(i.app_tp_I2C_init) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_st_touch.o(i.app_tp_phone_analysis_data_for_wake_up) for app_tp_phone_analysis_data_for_wake_up
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) for app_tp_phone_analysis_data
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(i.app_tp_s_read) for app_tp_s_read
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(i.app_tp_s_write) for app_tp_s_write
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_st_touch.o(.data) for g_tp_wakeup_response
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.app_tp_init) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    app_tp_transfer.o(i.app_tp_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    app_tp_transfer.o(i.app_tp_init) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_master.o(i.hal_i2c_m_dma_init) for hal_i2c_m_dma_init
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_for_custom_s8.o(.data) for g_phone_output_int_pad
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.app_tp_m_read) refers to hal_i2c_master.o(i.hal_i2c_m_dma_read) for hal_i2c_m_dma_read
    app_tp_transfer.o(i.app_tp_m_transfer_complate) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.app_tp_m_write) refers to hal_i2c_master.o(i.hal_i2c_m_dma_write) for hal_i2c_m_dma_write
    app_tp_transfer.o(i.app_tp_phone_clear_reset_on) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_phone_reset_on) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_s_read) refers to hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read) for hal_i2c_s_nonblocking_read
    app_tp_transfer.o(i.app_tp_s_transfer_complate) refers to hal_i2c_slave.o(i.hal_i2c_s_write_complate) for hal_i2c_s_write_complate
    app_tp_transfer.o(i.app_tp_s_transfer_complate) refers to hal_i2c_slave.o(i.hal_i2c_s_read_complate) for hal_i2c_s_read_complate
    app_tp_transfer.o(i.app_tp_s_write) refers to hal_i2c_slave.o(i.hal_i2c_s_dma_write) for hal_i2c_s_dma_write
    app_tp_transfer.o(i.app_tp_screen_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    app_tp_transfer.o(i.app_tp_screen_init) refers to tau_delay.o(i.delayUs) for delayUs
    app_tp_transfer.o(i.app_tp_screen_init) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_transfer.o(i.app_tp_screen_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_rst_pad
    app_tp_transfer.o(i.app_tp_screen_int_callback) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to hal_spi_master.o(i.hal_spi_m_clear_rxfifo) for hal_spi_m_clear_rxfifo
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(i.S20_Start_init) for S20_Start_init
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_for_custom_s8.o(.constdata) for screen_reg_start_data_size
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to ap_demo.o(.data) for phone_start_flag
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_st_touch.o(i.app_tp_screen_analysis_wake_up_exec) for app_tp_screen_analysis_wake_up_exec
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_transfer_screen_const) for app_tp_transfer_screen_const
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_F3) for ap_tp_st_touch_error_handler_F3
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_FF) for ap_tp_st_touch_error_handler_FF
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event) for ap_tp_st_touch_scan_point_record_event
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_st_touch.o(i.app_tp_screen_analysis_wake_up) for app_tp_screen_analysis_wake_up
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) for app_tp_screen_analysis_int
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to tau_delay.o(i.delayUs) for delayUs
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(.data) for screen_reg_int_data
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(.data) for tp_sleep_in
    app_tp_transfer.o(i.app_tp_transfer_screen_start) refers to app_tp_transfer.o(i.app_tp_transfer_screen_const) for app_tp_transfer_screen_const
    app_tp_transfer.o(i.app_tp_transfer_screen_start) refers to app_tp_transfer.o(.data) for .data
    app_tp_st_touch.o(i.CRC16_2) refers to app_tp_st_touch.o(.constdata) for .constdata
    app_tp_st_touch.o(i.ap_get_tp_calibration_status_01) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) for hal_dsi_rx_ctrl_send_ack_cmd
    app_tp_st_touch.o(i.ap_get_tp_calibration_status_01) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.ap_set_tp_calibration_04) refers to memseta.o(.text) for __aeabi_memclr4
    app_tp_st_touch.o(i.ap_set_tp_calibration_04) refers to printfa.o(i.__0printf) for __2printf
    app_tp_st_touch.o(i.ap_set_tp_calibration_04) refers to app_tp_st_touch.o(i.CRC16_2) for CRC16_2
    app_tp_st_touch.o(i.ap_set_tp_calibration_04) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.ap_tp_st_touch_calibration) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_st_touch.o(i.ap_tp_st_touch_calibration) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_st_touch.o(i.ap_tp_st_touch_calibration) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_calibration) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_F3) refers to app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) for ap_tp_st_touch_software_reset
    app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_FF) refers to app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) for ap_tp_st_touch_software_reset
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to memseta.o(.text) for __aeabi_memclr4
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to tau_log.o(i.LOG_printf) for LOG_printf
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_rst_pad
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init) refers to app_tp_st_touch.o(.bss) for .bss
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event) refers to app_tp_st_touch.o(.bss) for .bss
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec) refers to printfa.o(i.__0printf) for __2printf
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event) for ap_tp_st_touch_simulate_finger_release_event
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init) for ap_tp_st_touch_scan_point_init
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec) refers to app_tp_st_touch.o(.bss) for .bss
    app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event) refers to app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) for app_tp_screen_analysis_int
    app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event) for ap_tp_st_touch_simulate_finger_release_event
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init) for ap_tp_st_touch_scan_point_init
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_calibration) for ap_tp_st_touch_calibration
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) for ap_tp_st_touch_get_calibration_success_mark
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to tau_log.o(i.LOG_printf) for LOG_printf
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.app_tp_phone_analysis_data_for_wake_up) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_st_touch.o(i.app_tp_phone_analysis_data_for_wake_up) refers to app_tp_for_custom_s8.o(.data) for g_phone_output_int_pad
    app_tp_st_touch.o(i.app_tp_phone_analysis_data_for_wake_up) refers to app_tp_st_touch.o(.bss) for .bss
    app_tp_st_touch.o(i.app_tp_phone_analysis_data_for_wake_up) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.app_tp_screen_analysis_wake_up) refers to app_tp_st_touch.o(.bss) for .bss
    app_tp_st_touch.o(i.app_tp_screen_analysis_wake_up) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.app_tp_screen_analysis_wake_up_exec) refers to tau_log.o(i.LOG_printf) for LOG_printf
    app_tp_st_touch.o(i.app_tp_screen_analysis_wake_up_exec) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_st_touch.o(i.app_tp_screen_analysis_wake_up_exec) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.app_tp_screen_analysis_wake_up_exec) refers to app_tp_st_touch.o(.bss) for .bss
    app_tp_st_touch.o(i.app_tp_screen_analysis_wake_up_exec) refers to app_tp_for_custom_s8.o(.data) for g_phone_output_int_pad
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_init) for hal_system_init
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_enable_systick) for hal_system_enable_systick
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_init_console) for hal_system_init_console
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_set_phy_calibration) for hal_system_set_phy_calibration
    startup_armcm0.o(RESET) refers to startup_armcm0.o(STACK) for __initial_sp
    startup_armcm0.o(RESET) refers to startup_armcm0.o(.text) for Reset_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.HardFault_Handler) for HardFault_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SysTick_Handler) for SysTick_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.VIDC_IRQn_Handler) for VIDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.LCDC_IRQn_Handler) for LCDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.MIPI_RX_IRQn_Handler) for MIPI_RX_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.MIPI_TX_IRQn_Handler) for MIPI_TX_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.MEMC_IRQn_Handler) for MEMC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.VPRE_IRQn_Handler) for VPRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.FLSCTRL_IRQn_Handler) for FLSCTRL_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.DMA_IRQn_Handler) for DMA_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER0_IRQn_Handler) for TIMER0_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER1_IRQn_Handler) for TIMER1_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER2_IRQn_Handler) for TIMER2_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER3_IRQn_Handler) for TIMER3_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.WDG_IRQn_Handler) for WDG_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.UART_IRQn_Handler) for UART_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.I2C0_IRQn_Handler) for I2C0_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.I2C1_IRQn_Handler) for I2C1_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SPIS_IRQn_Handler) for SPIS_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SPIM_IRQn_Handler) for SPIM_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.ADC_IRQn_Handler) for ADC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.PWMDET_IRQn_Handler) for PWMDET_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SWIRE_IRQn_Handler) for SWIRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.AP_NRESET_IRQn_Handler) for AP_NRESET_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT0_IRQn_Handler) for EXTI_INT0_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT1_IRQn_Handler) for EXTI_INT1_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT2_IRQn_Handler) for EXTI_INT2_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT3_IRQn_Handler) for EXTI_INT3_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT4_IRQn_Handler) for EXTI_INT4_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT5_IRQn_Handler) for EXTI_INT5_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT6_IRQn_Handler) for EXTI_INT6_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT7_IRQn_Handler) for EXTI_INT7_IRQn_Handler
    startup_armcm0.o(.text) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to app_tp_for_custom_s8.o(.data) for .data
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to app_tp_for_custom_s8.o(.constdata) for .constdata
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to app_tp_transfer.o(i.app_tp_screen_init) for app_tp_screen_init
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to app_tp_for_custom_s8.o(.data) for .data
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to uidiv.o(.text) for __aeabi_uidivmod
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to app_tp_for_custom_s8.o(.data) for .data
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_1
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_2
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_3
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_4
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_5
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_6
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_7
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_point_data
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_point_back
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_coord_data
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_coord_back
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to drv_vidc.o(i.drv_vidc_set_module_enable) for drv_vidc_set_module_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) for hal_internal_vsync_get_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to hal_internal_vsync.o(i.hal_internal_rx_dcs_async_handler) for hal_internal_rx_dcs_async_handler
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to hal_internal_vsync.o(i.hal_internal_rx_dcs_polling) for hal_internal_rx_dcs_polling
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg) for drv_dsi_rx_set_ddi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_crgu.o(i.drv_crgu_set_rxbr_src) for drv_crgu_set_rxbr_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_crgu.o(i.drv_crgu_set_rxbr_div) for drv_crgu_set_rxbr_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg) for drv_dsi_rx_set_ipi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_gen_a_tear_signal) for drv_memc_gen_a_tear_signal
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size) for drv_dsi_rx_get_max_ret_size
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) for hal_dsi_rx_ctrl_init_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_rx) for hal_internal_vsync_init_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) for hal_dsi_rx_ctrl_init_dsi_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) for hal_dsi_rx_ctrl_init_rxbr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps) for drv_dsc_dec_set_u8_pps
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) for hal_dsi_rx_ctrl_init_vidc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) for hal_dsi_rx_ctrl_init_memc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_chip_info.o(i.drv_chip_rx_init_done) for drv_chip_rx_init_done
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_vidc_src) for drv_crgu_set_vidc_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_fb_src) for drv_crgu_set_fb_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_fb_div) for drv_crgu_set_fb_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) for hal_dsi_rx_ctrl_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg) for drv_dsi_rx_set_ctrl_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) for drv_dsi_rx_set_up_phy
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap) for drv_dsi_rx_set_lane_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_inten) for drv_dsi_rx_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt) for drv_dsi_rx_set_resp_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_mode) for drv_memc_set_ltpo_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tear_mode) for hal_internal_vsync_get_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_vsync.o(i.hal_internal_check_video_auto_sync) for hal_internal_check_video_auto_sync
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_fs_en_conditions) for drv_memc_set_fs_en_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_lcdc_st_conditions) for drv_memc_set_lcdc_st_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_vidc_sync_cnt) for drv_memc_set_vidc_sync_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_double_buffer) for drv_memc_set_double_buffer
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_active_height) for drv_memc_set_active_height
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_inten) for drv_memc_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_color_format) for drv_rxbr_set_color_format
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th) for drv_rxbr_set_ltpo_drop_th
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_cfg) for drv_rxbr_set_usr_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_col) for drv_rxbr_set_usr_col
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_row) for drv_rxbr_set_usr_row
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg) for drv_rxbr_hline_rcv_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) for hal_internal_vsync_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_src_parameter) for drv_vidc_set_src_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pentile_swap) for drv_vidc_set_pentile_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_dst_parameter) for drv_vidc_set_dst_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_init_module_enable) for drv_vidc_init_module_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_rotation) for drv_vidc_set_rotation
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_init_get_scld_filter_h) for drv_param_init_get_scld_filter_h
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_init_get_scld_filter_v) for drv_param_init_get_scld_filter_v
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef0) for drv_vidc_set_scld_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef1) for drv_vidc_set_scld_hcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef0) for drv_vidc_set_scld_vcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef1) for drv_vidc_set_scld_vcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_p2r_hinitr) for drv_vidc_set_p2r_hinitr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_p2r_hinitb) for drv_vidc_set_p2r_hinitb
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_p2r_filter_init) for drv_param_p2r_filter_init
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_p2r_hcoef0) for drv_vidc_set_p2r_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_mirror) for drv_vidc_set_mirror
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pu_ctrl) for drv_vidc_set_pu_ctrl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter) for drv_dsc_dec_convert_pps_rc_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_write_cmd_entry) refers to hal_internal_vsync.o(i.hal_internal_vsync_register_write_cmd_entry) for hal_internal_vsync_register_write_cmd_entry
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header) for drv_rxbr_set_ack_pkt_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) for hal_internal_vsync_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef0) for drv_vidc_set_scld_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef1) for drv_vidc_set_scld_hcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef0) for drv_vidc_set_scld_vcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef1) for drv_vidc_set_scld_vcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_param_init.o(i.drv_param_init_set_scld_filter) for drv_param_init_set_scld_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) for hal_internal_vsync_set_sync_line
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg) for drv_rxbr_hline_rcv0_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_dcs_direct_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode) for hal_internal_vsync_set_dcs_direct_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) refers to drv_rxbr.o(i.drv_rxbr_set_cmd_filter) for drv_rxbr_set_cmd_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) for drv_dsi_rx_calc_ipi_tx_delay
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg) for drv_dsi_rx_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format) refers to drv_vidc.o(i.drv_vidc_update_src_format) for drv_vidc_update_src_format
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format) refers to drv_vidc.o(i.drv_vidc_set_pentile_swap) for drv_vidc_set_pentile_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dflti.o(.text) for __aeabi_i2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dmul.o(.text) for __aeabi_dmul
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to ddiv.o(.text) for __aeabi_ddiv
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to dflti.o(.text) for __aeabi_i2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to dmul.o(.text) for __aeabi_dmul
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to ddiv.o(.text) for __aeabi_ddiv
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) for hal_dsi_rx_ctrl_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk) for hal_intl_svs_update_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_src) for drv_crgu_set_rxbr_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_div) for drv_crgu_set_rxbr_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_dsco_src) for drv_crgu_set_dsco_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_dsco_src_div) for drv_crgu_set_dsco_src_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_dsc_core_div) for drv_crgu_set_dsc_core_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_te_waveform) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_te_waveform) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_dsi_rx.o(i.drv_dsi_rx_power_up) for drv_dsi_rx_power_up
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) for hal_internal_vsync_toggle_input_frame_rate
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) for hal_internal_sync_input_resolution_change
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution_ex) refers to hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) for hal_internal_sync_input_resolution_change_ex
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution_ex) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fscalb.o(.text) for __ARM_scalbnf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fflti.o(.text) for __aeabi_i2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to ffixi.o(.text) for __aeabi_f2iz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk) for drv_dsi_tx_set_video_chunk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing) for drv_dsi_tx_set_video_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to drv_phy_common.o(i.drv_phy_get_rate_para) for drv_phy_get_rate_para
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to ffixui.o(.text) for __aeabi_f2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to hal_dsi_tx_ctrl.o(.conststring) for .conststring
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) for hal_lcdc_config_upscaler
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to drv_lcdc.o(i.drv_lcdc_config_src_parameter) for drv_lcdc_config_src_parameter
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to hal_internal_vsync.o(i.hal_internal_vsync_update_lcdc_addr) for hal_internal_vsync_update_lcdc_addr
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode_rcv_te) refers to hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) for hal_internal_sync_cmd_mode_rcv_te
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_param_init.o(i.drv_param_init_set_ccm) for drv_param_init_set_ccm
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.constdata) for .constdata
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) for hal_lcdc_config_upscaler
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) for hal_lcdc_config_remains
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_mode_init) for hal_dsi_tx_ctrl_draw_mode_init
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) for hal_dsi_tx_ctrl_set_rect_pixel_data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) for hal_lcdc_config_upscaler
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) for hal_lcdc_config_remains
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_mode_init) for hal_dsi_tx_ctrl_draw_mode_init
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_ulps_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) for drv_dsi_tx_phy_ulps_enter
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_ulps_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) for drv_dsi_tx_phy_ulps_exit
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) for hal_dsi_tx_ctrl_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_tx) for hal_internal_vsync_init_tx
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate) for hal_dsi_tx_config_params_for_lane_rate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) for hal_dsi_tx_count_lane_rate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) for hal_dsi_tx_init_phy_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) for drv_dsi_tx_phy_test_setup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) for hal_lcdc_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) for hal_lcdc_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) for hal_dsi_tx_init_dpi_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) for hal_dsi_tx_init_data_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) for hal_dsi_tx_init_remains
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt) for hal_dsi_tx_init_interrupt
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready) for drv_dsi_tx_phy_status_ready
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload) for drv_dsi_tx_command_get_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) refers to drv_param_init.o(i.drv_param_init_set_ccm) for drv_param_init_set_ccm
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_pq_filter) refers to drv_lcdc.o(i.drv_lcdc_config_scale_up_coef) for drv_lcdc_config_scale_up_coef
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_pq_filter) refers to drv_param_init.o(i.drv_param_init_set_sclu_filter) for drv_param_init_set_sclu_filter
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness) refers to drv_lcdc.o(i.drv_lcdc_config_endianness) for drv_lcdc_config_endianness
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_lp_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd) for drv_dsi_tx_video_mode_set_lp_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb) for drv_lcdc_config_overwrite_rgb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp) refers to drv_lcdc.o(i.drv_lcdc_config_partial_display_enable) for drv_lcdc_config_partial_display_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area) refers to drv_lcdc.o(i.drv_lcdc_config_partial_display_area) for drv_lcdc_config_partial_display_area
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to dflti.o(.text) for __aeabi_i2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to dmul.o(.text) for __aeabi_dmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to ddiv.o(.text) for __aeabi_ddiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_vpg) for drv_dsi_tx_set_vpg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) for hal_dsi_tx_ctrl_draw_flicker
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) for hal_dsi_tx_ctrl_draw_chessboard
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_enable_shadow_reg) for drv_lcdc_enable_shadow_reg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_check_video_auto_sync) for hal_internal_check_video_auto_sync
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_start) for drv_lcdc_start
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_set_video_hw_mode) for drv_lcdc_set_video_hw_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size) for drv_dsi_tx_edpi_cmd_size
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) for hal_dsi_tx_init_video_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode) for drv_dsi_tx_dpi_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity) for drv_dsi_tx_dpi_polarity
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time) for drv_dsi_tx_dpi_lpcmd_time
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_int) for drv_dsi_tx_config_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode) for drv_dsi_tx_phy_lane_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg) for drv_dsi_tx_phy_time_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_response_mode) for drv_dsi_tx_response_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div) for drv_dsi_tx_set_time_out_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg) for drv_dsi_tx_timeout_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp) for drv_dsi_tx_phy_clock_lane_auto_lp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg) for drv_dsi_tx_video_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack) for drv_dsi_tx_set_bta_ack
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd) for drv_dsi_tx_video_mode_set_lp_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_disable_hact_cmd) for drv_dsi_tx_video_mode_disable_hact_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) for hal_dsi_tx_calc_video_chunks
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_header) for drv_dsi_tx_command_header
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) refers to drv_param_init.o(i.drv_param_init_get_ccm) for drv_param_init_get_ccm
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) refers to drv_lcdc.o(i.drv_lcdc_config_ccm) for drv_lcdc_config_ccm
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to hal_internal_vsync.o(i.hal_internal_check_video_auto_sync) for hal_internal_check_video_auto_sync
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_disp_mode) for drv_lcdc_config_disp_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_edpi_mode) for drv_lcdc_config_edpi_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_endianness) for drv_lcdc_config_endianness
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_thresh) for drv_lcdc_config_thresh
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_dpi_polarity) for drv_lcdc_config_dpi_polarity
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_src_parameter) for drv_lcdc_config_src_parameter
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area) for hal_dsi_tx_ctrl_set_partial_disp_area
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp) for hal_dsi_tx_ctrl_set_partial_disp
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_lcdc.o(i.drv_lcdc_config_scale_up_step) for drv_lcdc_config_scale_up_step
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_param_init.o(i.drv_param_init_get_sclu_filter) for drv_param_init_get_sclu_filter
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_lcdc.o(i.drv_lcdc_config_scale_up_coef) for drv_lcdc_config_scale_up_coef
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) for hal_lcdc_config_upscaler
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) for hal_lcdc_config_ccm
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile) for hal_lcdc_config_rgb_to_pentile
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) for hal_lcdc_config_remains
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) for hal_lcdc_init_interrupt
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to drv_lcdc.o(i.drv_lcdc_set_prefetch) for drv_lcdc_set_prefetch
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dpi_pre_div) for drv_crgu_set_dpi_pre_div
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dpi_pre_src) for drv_crgu_set_dpi_pre_src
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dpi_mux_src) for drv_crgu_set_dpi_mux_src
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_lcdc.o(i.drv_lcdc_config_dpi_timing) for drv_lcdc_config_dpi_timing
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to hal_internal_vsync.o(i.hal_internal_check_video_auto_sync) for hal_internal_check_video_auto_sync
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to hal_internal_soft_sync.o(i.hal_intl_svs_init_tx) for hal_intl_svs_init_tx
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to cfrcmple.o(.text) for __aeabi_cfrcmple
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ffixi.o(.text) for __aeabi_f2iz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_lcdc_div) for drv_crgu_set_lcdc_div
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_lcdc_src) for drv_crgu_set_lcdc_src
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) for hal_tx_frame_rate_adjust
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to drv_lcdc.o(i.drv_lcdc_ctrl_flow) for drv_lcdc_ctrl_flow
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to drv_lcdc.o(i.drv_lcdc_config_int) for drv_lcdc_config_int
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to cfcmple.o(.text) for __aeabi_cfcmple
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_gpio.o(i.hal_gpio_ctrl_eint) refers to drv_gpio.o(i.drv_gpio_set_int) for drv_gpio_set_int
    hal_gpio.o(i.hal_gpio_ctrl_eint) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_get_input_data) refers to drv_gpio.o(i.drv_gpio_get_input_data) for drv_gpio_get_input_data
    hal_gpio.o(i.hal_gpio_get_int_type) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to drv_gpio.o(i.drv_gpio_get_pull_state) for drv_gpio_get_pull_state
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_eint) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group) for drv_sys_cfg_sel_gpio_group
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig) for drv_sys_cfg_sel_int_trig
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_init_eint) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_input) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_input) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_input) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_init_output) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_reg_eint_cb) refers to drv_gpio.o(i.drv_gpio_register_callback) for drv_gpio_register_callback
    hal_gpio.o(i.hal_gpio_reg_eint_cb) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_gpio.o(i.drv_gpio_register_ap_reset_callback) for drv_gpio_register_ap_reset_callback
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) for drv_sys_cfg_sel_ap_rst_trig
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to drv_gpio.o(i.drv_gpio_set_driving_strength) for drv_gpio_set_driving_strength
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode3) for drv_gpio_set_mode3
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode2) for drv_gpio_set_mode2
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode1) for drv_gpio_set_mode1
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode0) for drv_gpio_set_mode0
    hal_gpio.o(i.hal_gpio_set_mode) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_output_data) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to drv_gpio.o(i.drv_gpio_set_pull_state) for drv_gpio_set_pull_state
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to drv_gpio.o(i.drv_gpio_set_schmitt_trigger) for drv_gpio_set_schmitt_trigger
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to drv_gpio.o(i.drv_gpio_set_slew_rate) for drv_gpio_set_slew_rate
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to hal_gpio.o(.constdata) for .constdata
    hal_i2c_master.o(i.hal_i2c_m_deinit) refers to drv_i2c_master.o(i.drv_i2c_m_deinit) for drv_i2c_m_deinit
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_master.o(i.drv_i2c_master_init) for drv_i2c_master_init
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_master.o(i.drv_i2c1_set_callback) for drv_i2c1_set_callback
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_master.o(i.drv_i2c_m_enable_intr) for drv_i2c_m_enable_intr
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_dma.o(i.drv_i2c_dma_init) for drv_i2c_dma_init
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_dma.o(i.drv_i2c_enable_rx_dma) for drv_i2c_enable_rx_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_dma.o(i.drv_i2c_enable_tx_dma) for drv_i2c_enable_tx_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to hal_i2c_master.o(i.hal_i2c_master_irq_callback) for hal_i2c_master_irq_callback
    hal_i2c_master.o(i.hal_i2c_m_dma_read) refers to drv_i2c_dma.o(i.drv_i2c_master_read_dma) for drv_i2c_master_read_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_read) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_master.o(i.hal_i2c_m_dma_write) refers to drv_i2c_dma.o(i.drv_i2c_master_write_dma) for drv_i2c_master_write_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_write) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_master.o(i.hal_i2c_m_set_high_impedance) refers to drv_i2c_master.o(i.drv_i2c_m_enable) for drv_i2c_m_enable
    hal_i2c_master.o(i.hal_i2c_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_master.o(i.hal_i2c_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_i2c_master.o(i.hal_i2c_m_transfer_complate) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_master.o(i.hal_i2c_master_irq_callback) refers to drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit) for drv_i2c_m_clear_it_pending_bit
    hal_i2c_master.o(i.hal_i2c_master_irq_callback) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to drv_i2c_slave.o(i.drv_i2c_s_set_intr) for drv_i2c_s_set_intr
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to drv_i2c_slave.o(i.drv_i2c_s_enable) for drv_i2c_s_enable
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to drv_i2c_dma.o(i.drv_i2c_slave_write_dma) for drv_i2c_slave_write_dma
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_get_tx_byte_num) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c_slave_init) for drv_i2c_slave_init
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_master.o(i.drv_i2c1_set_callback) for drv_i2c1_set_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c_s_config_intr) for drv_i2c_s_config_intr
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c_s_set_intr) for drv_i2c_s_set_intr
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_dma.o(i.drv_i2c_dma_init) for drv_i2c_dma_init
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) for drv_i2c_set_dma_irq_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_dma.o(i.drv_i2c_enable_tx_dma) for drv_i2c_enable_tx_dma
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c0_set_callback) for drv_i2c0_set_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) for hal_i2c_slave_irq_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback) for hal_i2c_s_dma_user_callback
    hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_complate) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_complate_clear) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_data) refers to drv_i2c_slave.o(i.drv_i2c_s_read_data) for drv_i2c_s_read_data
    hal_i2c_slave.o(i.hal_i2c_s_read_data) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_data) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_rxfifo_notempty) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    hal_i2c_slave.o(i.hal_i2c_s_rxfifo_notempty) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_rxfifo_notempty) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_sel) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_set_dma_tx_cycle) refers to drv_dma.o(i.drv_dma_enable_cycle) for drv_dma_enable_cycle
    hal_i2c_slave.o(i.hal_i2c_s_set_dma_tx_cycle) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_set_dma_tx_cycle) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to drv_i2c_slave.o(i.drv_i2c_s_enable) for drv_i2c_s_enable
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_set_transfer) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_write_complate) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_write_data) refers to drv_i2c_slave.o(i.drv_i2c_s_write_data) for drv_i2c_s_write_data
    hal_i2c_slave.o(i.hal_i2c_s_write_data) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_write_data) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit) for drv_i2c_s_clear_it_pending_bit
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(i.drv_i2c_s_write_data) for drv_i2c_s_write_data
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_spi_master.o(i.hal_spi_m_callback) refers to drv_spi_dma.o(i.drv_spi_abort_dma) for drv_spi_abort_dma
    hal_spi_master.o(i.hal_spi_m_callback) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_clear_rxfifo) refers to drv_spi_master.o(i.drv_spi_m_read_data) for drv_spi_m_read_data
    hal_spi_master.o(i.hal_spi_m_deinit) refers to drv_spi_master.o(i.drv_spi_m_deinit) for drv_spi_m_deinit
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to hal_spi_master.o(i.hal_spi_m_gpio_init) for hal_spi_m_gpio_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_master.o(i.drv_spi_master_init) for drv_spi_master_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_dma_init) for drv_spi_dma_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_dma_ch6_init) for drv_spi_dma_ch6_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) for drv_spi_set_dma_irq_callback
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) for drv_spi_set_dma_ch6_irq_callback
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req) for drv_sys_cfg_set_dma_rx_req
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_master.o(i.drv_spi_m_enable_rx_dma) for drv_spi_m_enable_rx_dma
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to hal_spi_master.o(i.hal_spi_m_callback) for hal_spi_m_callback
    hal_spi_master.o(i.hal_spi_m_dma_read) refers to drv_spi_dma.o(i.drv_spim_dma_read) for drv_spim_dma_read
    hal_spi_master.o(i.hal_spi_m_dma_read) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_dma_write) refers to drv_spi_dma.o(i.drv_spim_dma_write) for drv_spim_dma_write
    hal_spi_master.o(i.hal_spi_m_dma_write) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_get_transfer_complate) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_gpio_init) refers to drv_spi_master.o(i.drv_spi_m_gpio_init) for drv_spi_m_gpio_init
    hal_spi_master.o(i.hal_spi_m_read_rxfifo) refers to drv_spi_master.o(i.drv_spi_m_read_data) for drv_spi_m_read_data
    hal_spi_master.o(i.hal_spi_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_spi_master.o(i.hal_spi_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    hal_spi_master.o(i.hal_spi_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_system.o(i.hal_system_deep_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode) for drv_pwr_enter_deep_sleep_mode
    hal_system.o(i.hal_system_disable_systick) refers to drv_common.o(i.drv_common_disable_systick) for drv_common_disable_systick
    hal_system.o(i.hal_system_enable_systick) refers to drv_common.o(i.drv_common_enable_systick) for drv_common_enable_systick
    hal_system.o(i.hal_system_get_tick) refers to drv_common.o(i.drv_common_get_tick) for drv_common_get_tick
    hal_system.o(i.hal_system_idle_mode) refers to drv_common.o(i.drv_common_idle_mode) for drv_common_idle_mode
    hal_system.o(i.hal_system_init) refers to drv_pwr.o(i.drv_pwr_set_system_clk_src) for drv_pwr_set_system_clk_src
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_set_ahb_src) for drv_crgu_set_ahb_src
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_set_ahb_pre_div) for drv_crgu_set_ahb_pre_div
    hal_system.o(i.hal_system_init) refers to irq_redirect .o(i.handle_init) for handle_init
    hal_system.o(i.hal_system_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int) for drv_sys_cfg_clear_all_int
    hal_system.o(i.hal_system_init) refers to drv_common.o(i.drv_common_system_init) for drv_common_system_init
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_system.o(i.hal_system_init) refers to drv_pwr.o(i.drv_pwr_set_pvd_mode) for drv_pwr_set_pvd_mode
    hal_system.o(i.hal_system_init) refers to drv_common.o(.data) for g_system_clock
    hal_system.o(i.hal_system_init_console) refers to hal_uart.o(i.hal_uart_init) for hal_uart_init
    hal_system.o(i.hal_system_register_systick_cb) refers to drv_common.o(i.drv_common_systick_register_cb) for drv_common_systick_register_cb
    hal_system.o(i.hal_system_set_phy_calibration) refers to drv_phy_common.o(i.drv_phy_enable_calibration) for drv_phy_enable_calibration
    hal_system.o(i.hal_system_set_pvd) refers to drv_pwr.o(i.drv_pwr_set_pvd_mode) for drv_pwr_set_pvd_mode
    hal_system.o(i.hal_system_set_vcc) refers to drv_pwr.o(i.drv_pwr_set_cp_mode) for drv_pwr_set_cp_mode
    hal_system.o(i.hal_system_share_flash_mode) refers to drv_fls.o(i.drv_fls_gpio_connect) for drv_fls_gpio_connect
    hal_system.o(i.hal_system_share_flash_mode) refers to drv_fls.o(i.drv_fls_gpio_disconnect) for drv_fls_gpio_disconnect
    hal_system.o(i.hal_system_sleep_mode) refers to drv_crgu.o(i.drv_crgu_config_clocks) for drv_crgu_config_clocks
    tau_delay.o(i.delayMs) refers to tau_delay.o(i.delayUs) for delayUs
    tau_log.o(i.LOG_printf) refers to printfa.o(i.__0vsprintf) for vsprintf
    tau_log.o(i.LOG_printf) refers to printfa.o(i.__0printf) for __2printf
    tau_log.o(i.LOG_printf) refers to tau_log.o(.bss) for .bss
    tau_log.o(i.fgetc) refers to hal_uart.o(i.hal_uart_receive_blocking) for hal_uart_receive_blocking
    tau_log.o(i.fputc) refers to hal_uart.o(i.hal_uart_transmit_blocking) for hal_uart_transmit_blocking
    hal_uart.o(i.hal_uart_deinit) refers to drv_dma.o(i.drv_dma_deinit) for drv_dma_deinit
    hal_uart.o(i.hal_uart_deinit) refers to drv_uart.o(i.UART_Deinit) for UART_Deinit
    hal_uart.o(i.hal_uart_dmacallback) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_uart.o(i.hal_uart_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_uart.o(i.hal_uart_init) refers to drv_uart.o(i.UART_init) for UART_init
    hal_uart.o(i.hal_uart_init) refers to drv_common.o(.data) for g_system_clock
    hal_uart.o(i.hal_uart_init) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_receive_blocking) refers to drv_uart.o(i.UART_ReadBlocking) for UART_ReadBlocking
    hal_uart.o(i.hal_uart_receive_dma) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    hal_uart.o(i.hal_uart_receive_dma) refers to drv_uart_dma.o(i.UART_TransferCreateHandleDMA) for UART_TransferCreateHandleDMA
    hal_uart.o(i.hal_uart_receive_dma) refers to drv_uart_dma.o(i.UART_TransferReceiveDMA) for UART_TransferReceiveDMA
    hal_uart.o(i.hal_uart_receive_dma) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_receive_dma) refers to hal_uart.o(i.hal_uart_dmacallback) for hal_uart_dmacallback
    hal_uart.o(i.hal_uart_transmit_blocking) refers to drv_uart.o(i.UART_WriteBlocking) for UART_WriteBlocking
    hal_uart.o(i.hal_uart_transmit_dma) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    hal_uart.o(i.hal_uart_transmit_dma) refers to drv_uart_dma.o(i.UART_TransferCreateHandleDMA) for UART_TransferCreateHandleDMA
    hal_uart.o(i.hal_uart_transmit_dma) refers to drv_uart_dma.o(i.UART_TransferSendDMA) for UART_TransferSendDMA
    hal_uart.o(i.hal_uart_transmit_dma) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_transmit_dma) refers to hal_uart.o(i.hal_uart_dmacallback) for hal_uart_dmacallback
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_param_init.o(i.drv_param_init_get_ccm) for drv_param_init_get_ccm
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_lcdc.o(i.drv_lcdc_config_ccm) for drv_lcdc_config_ccm
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to ddiv.o(.text) for __aeabi_ddiv
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to sqrt.o(i.sqrt) for sqrt
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to dmul.o(.text) for __aeabi_dmul
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to cdcmple.o(.text) for __aeabi_cdcmple
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to hal_internal_vsync.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_get_pkt_buf_error_status) for drv_rxbr_get_pkt_buf_error_status
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.dcs_sw_filter) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.dcs_sw_filter) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_check_video_auto_sync) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tear_mode) for hal_internal_vsync_get_tear_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_mode) for drv_memc_set_ltpo_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_double_buffer) for drv_memc_set_double_buffer
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_active_height) for drv_memc_set_active_height
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_inten) for drv_memc_set_inten
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_rx_dcs_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) for dcs_packet_get_fifo_header
    hal_internal_vsync.o(i.hal_internal_rx_dcs_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) for dcs_packet_free_fifo_header
    hal_internal_vsync.o(i.hal_internal_rx_dcs_polling) refers to hal_internal_vsync.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_vsync.o(i.hal_internal_rx_dcs_polling) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_bta_status) for drv_dsi_rx_get_bta_status
    hal_internal_vsync.o(i.hal_internal_rx_dcs_polling) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.hal_internal_rx_dcs_polling) refers to hal_internal_vsync.o(i.drv_rxbr_get_status1) for drv_rxbr_get_status1
    hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) refers to drv_lcdc.o(i.drv_lcdc_start) for drv_lcdc_start
    hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) for hal_dsi_rx_ctrl_gen_a_tear_signal
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_delay.o(i.delayUs) for delayUs
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.hal_internal_init_memc) for hal_internal_init_memc
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to drv_lcdc.o(i.drv_lcdc_enable_shadow_reg) for drv_lcdc_enable_shadow_reg
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to tau_delay.o(i.delayMs) for delayMs
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) for hal_dsi_rx_ctrl_gen_a_tear_signal
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to tau_delay.o(i.delayUs) for delayUs
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) for hal_vsync_reset_lcdc_scaler
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_internal_vsync.o(i.vsync_set_te_mode) for vsync_set_te_mode
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_tear_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_chip_info.o(i.drv_chip_rx_info_check) for drv_chip_rx_info_check
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_soft_sync.o(i.hal_intl_svs_init_rx) for hal_intl_svs_init_rx
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_rxbr.o(i.drv_rxbr_register_irq0_callback) for drv_rxbr_register_irq0_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_rxbr.o(i.drv_rxbr_register_irq1_callback) for drv_rxbr_register_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_vidc.o(i.drv_vidc_register_callback) for drv_vidc_register_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_init) for dcs_packet_fifo_init
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_gen_te) for soft_gen_te
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_gen_te_double_buffer) for soft_gen_te_double_buffer
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.rxbr_irq0_callback) for rxbr_irq0_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.rxbr_irq1_callback) for rxbr_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.vidc_callback) for vidc_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_register_write_cmd_entry) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) refers to memseta.o(.text) for __aeabi_memset
    hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) refers to drv_rxbr.o(i.drv_rxbr_set_filter_regs) for drv_rxbr_set_filter_regs
    hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) for hal_internal_vsync_set_auto_hw_filter
    hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_soft_sync.o(i.hal_intl_svs_deinit_tx) for hal_intl_svs_deinit_tx
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_soft_sync.o(i.hal_intl_svs_set_sync_coef) for hal_intl_svs_set_sync_coef
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(i.vsync_set_te_mode) for vsync_set_te_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_soft_sync.o(i.hal_intl_svs_deinit_tx) for hal_intl_svs_deinit_tx
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.vsync_set_te_mode) for vsync_set_te_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_soft_sync.o(i.hal_intl_svs_set_input_frate) for hal_intl_svs_set_input_frate
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg) for drv_rxbr_hline_rcv0_cfg
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_update_lcdc_addr) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dadd.o(.text) for __aeabi_dadd
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area) for hal_dsi_tx_ctrl_set_partial_disp_area
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp) for hal_dsi_tx_ctrl_set_partial_disp
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to drv_param_init.o(i.drv_param_init_get_sclu_filter) for drv_param_init_get_sclu_filter
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to drv_lcdc.o(i.drv_lcdc_config_scale_up_coef) for drv_lcdc_config_scale_up_coef
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_internal_vsync.o(i.hal_internal_init_memc) for hal_internal_init_memc
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(i.dcs_sw_filter) for dcs_sw_filter
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) for dcs_packet_fifo_alloc
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(i.hal_internal_rx_dcs_async_handler) for hal_internal_rx_dcs_async_handler
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_rxbr.o(i.drv_rxbr_get_col_addr) for drv_rxbr_get_col_addr
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_rxbr.o(i.drv_rxbr_get_page_addr) for drv_rxbr_get_page_addr
    hal_internal_vsync.o(i.rx_partial_update) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_dsc_dec.o(i.drv_dsc_dec_get_nslc) for drv_dsc_dec_get_nslc
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_crgu.o(i.drv_crgu_set_dsco_src) for drv_crgu_set_dsco_src
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_crgu.o(i.drv_crgu_set_dsco_src_div) for drv_crgu_set_dsco_src_div
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_crgu.o(i.drv_crgu_set_dsc_core_div) for drv_crgu_set_dsc_core_div
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rx_partial_update) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(i.rx_get_dcs_packet_data) for rx_get_dcs_packet_data
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(i.rx_receive_pps) for rx_receive_pps
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(i.drv_rxbr_get_status1) for drv_rxbr_get_status1
    hal_internal_vsync.o(i.rx_receive_packet) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_bta_status) for drv_dsi_rx_get_bta_status
    hal_internal_vsync.o(i.rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_get_pkt_buf_error_status) for drv_rxbr_get_pkt_buf_error_status
    hal_internal_vsync.o(i.rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_receive_pps) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.rx_receive_pps) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rx_receive_pps) refers to hal_internal_vsync.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter) for drv_dsc_dec_convert_pps_rc_parameter
    hal_internal_vsync.o(i.rx_receive_pps) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps) for drv_dsc_dec_set_u8_pps
    hal_internal_vsync.o(i.rx_receive_pps) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.rx_receive_pps) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_int_source) for drv_rxbr_get_int_source
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.rx_receive_packet) for rx_receive_packet
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.vpre_err_reset) for vpre_err_reset
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.rx_partial_update) for rx_partial_update
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_int_source) for drv_rxbr_get_int_source
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_soft_sync.o(i.hal_intl_svs_handle) for hal_intl_svs_handle
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.vpre_err_reset) for vpre_err_reset
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_lcdc.o(i.drv_lcdc_start) for drv_lcdc_start
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_memc.o(i.drv_memc_set_double_buffer_reverse) for drv_memc_set_double_buffer_reverse
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.soft_gen_te_double_buffer) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_gen_te_double_buffer) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_get_irq_status) for drv_vidc_get_irq_status
    hal_internal_vsync.o(i.vidc_callback) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_internal_vsync.o(i.vidc_callback) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_clear_irq) for drv_vidc_clear_irq
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_internal_vsync.o(i.vidc_callback) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps) for drv_dsc_dec_set_u8_pps
    hal_internal_vsync.o(i.vpre_err_reset) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to drv_lcdc.o(i.drv_lcdc_ctrl_flow) for drv_lcdc_ctrl_flow
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(.data) refers to hal_internal_vsync.o(.bss) for sg_te_info
    drv_common.o(i.app_HardFault_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_common.o(i.app_SysTick_Handler) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_enable_systick) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_common.o(i.drv_common_enable_systick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_get_tick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_system_init) refers to drv_chip_info.o(i.drv_chip_info_init) for drv_chip_info_init
    drv_common.o(i.drv_common_systick_register_cb) refers to drv_common.o(.data) for .data
    drv_dma.o(i.app_dma_irq_handler) refers to drv_dma.o(i.drv_dma_irq_handler) for drv_dma_irq_handler
    drv_dma.o(i.drv_dma_abort_transfer) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_abort_transfer) refers to drv_dma.o(i.drv_dma_disenable_channel_interrupts) for drv_dma_disenable_channel_interrupts
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_disenable_channel_interrupts) for drv_dma_disenable_channel_interrupts
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_clear_flag) for drv_dma_clear_flag
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_set_ccr) for drv_dma_set_ccr
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_dma.o(i.drv_dma_clear_flag) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.drv_dma_create_handle) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dma.o(i.drv_dma_disenable_channel_interrupts) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.drv_dma_enable_channel_interrupts) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dma.o(i.drv_dma_enable_cycle) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_get_remaining_bytes) refers to drv_dma.o(i.drv_dma_channel_is_active) for drv_dma_channel_is_active
    drv_dma.o(i.drv_dma_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dma.o(i.drv_dma_init) refers to drv_dma.o(i.drv_dma_ahb_init) for drv_dma_ahb_init
    drv_dma.o(i.drv_dma_irq_handler) refers to drv_dma.o(i.drv_dma_get_channel_flag) for drv_dma_get_channel_flag
    drv_dma.o(i.drv_dma_irq_handler) refers to drv_dma.o(i.drv_dma_clear_flag) for drv_dma_clear_flag
    drv_dma.o(i.drv_dma_irq_handler) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_m2m_init) refers to memseta.o(.text) for __aeabi_memclr4
    drv_dma.o(i.drv_dma_m2m_init) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    drv_dma.o(i.drv_dma_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_dma.o(i.drv_dma_set_burst) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_set_transfer) refers to drv_dma.o(i.drv_dma_set_burst) for drv_dma_set_burst
    drv_dma.o(i.drv_dma_start_transfer) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    drv_dma.o(i.drv_dma_start_transfer) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_fls.o(i.drv_fls_gpio_connect) refers to drv_fls.o(i.drv_fls_gpio_disconnect) for drv_fls_gpio_disconnect
    drv_fls.o(i.drv_fls_gpio_disconnect) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_EnableClk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_busy_pending) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    drv_fls.o(i.fls_de_init) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    drv_fls.o(i.fls_de_init) refers to drv_dma.o(i.drv_dma_clear_flag) for drv_dma_clear_flag
    drv_fls.o(i.fls_de_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_disable_it) refers to drv_fls.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_fls.o(i.fls_disable_it) refers to drv_fls.o(i.fls_set_mc_irq_mask) for fls_set_mc_irq_mask
    drv_fls.o(i.fls_enable_it) refers to drv_fls.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_fls.o(i.fls_enable_it) refers to drv_fls.o(i.fls_set_mc_irq_mask) for fls_set_mc_irq_mask
    drv_fls.o(i.fls_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_init) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_spi_init) for fls_spi_init
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_ctrl_cfg_init) for fls_ctrl_cfg_init
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_set_tuning) for fls_set_tuning
    drv_fls.o(i.fls_init) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_enable_it) for fls_enable_it
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_set_mc_irq_mask) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_fls.o(i.fls_set_mc_irq_mask) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_set_write) for fls_set_write
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_set_write) for fls_set_write
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect) for drv_ap_rst_trig_edge_detect
    drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_get_pull_state) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_register_ap_reset_callback) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.drv_gpio_register_callback) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_set_driving_strength) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.drv_gpio_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_gpio.o(i.drv_gpio_set_pull_state) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_set_schmitt_trigger) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_set_slew_rate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_i2c_dma.o(i.drv_i2c_dma_callback) refers to drv_i2c_dma.o(.data) for .data
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_i2c_master.o(i.drv_i2c_m_enable) for drv_i2c_m_enable
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req) for drv_sys_cfg_set_dma_rx_req
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_dma.o(i.drv_dma_set_transfer) for drv_dma_set_transfer
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_i2c_dma.o(i.drv_i2c_master_write_read_cmd) for drv_i2c_master_write_read_cmd
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_dma.o(i.drv_dma_set_transfer) for drv_dma_set_transfer
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_i2c_dma.o(.data) for .data
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_i2c_dma.o(.bss) for .bss
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_i2c_dma.o(i.drv_i2c_dma_callback) for drv_i2c_dma_callback
    drv_i2c_dma.o(i.drv_i2c_slave_write_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_i2c_master.o(i.app_I2C1_IRQn_Handler) refers to drv_i2c_master.o(.data) for .data
    drv_i2c_master.o(i.drv_i2c1_set_callback) refers to drv_i2c_master.o(.data) for .data
    drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_deinit) refers to drv_i2c_master.o(i.drv_i2c_m_disable_intr) for drv_i2c_m_disable_intr
    drv_i2c_master.o(i.drv_i2c_m_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_i2c_master.o(i.drv_i2c_m_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_i2c_master.o(i.drv_i2c_m_deinit) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_enable_intr) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_read_data) refers to drv_i2c_master.o(i.drv_i2c_m_get_fifo_status) for drv_i2c_m_get_fifo_status
    drv_i2c_master.o(i.drv_i2c_m_set_sys_mask) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_write_data) refers to drv_i2c_master.o(i.drv_i2c_m_get_fifo_status) for drv_i2c_m_get_fifo_status
    drv_i2c_master.o(i.drv_i2c_master_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_i2c_master.o(i.drv_i2c_master_init) refers to drv_common.o(.data) for g_system_clock
    drv_i2c_slave.o(i.app_I2C0_IRQn_Handler) refers to drv_i2c_slave.o(.data) for .data
    drv_i2c_slave.o(i.drv_i2c0_set_callback) refers to drv_i2c_slave.o(.data) for .data
    drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_i2c_slave.o(i.drv_i2c_s_read_data) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    drv_i2c_slave.o(i.drv_i2c_s_set_intr) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_i2c_slave.o(i.drv_i2c_s_set_intr) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_i2c_slave.o(i.drv_i2c_s_write_data) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    drv_i2c_slave.o(i.drv_i2c_slave_init) refers to drv_i2c_slave.o(i.drv_i2c_s_enable) for drv_i2c_s_enable
    drv_param_init.o(i.drv_param_init_get_ccm) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_get_scld_filter_h) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_get_scld_filter_v) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_get_sclu_filter) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_set_ccm) refers to memcpya.o(.text) for __aeabi_memcpy4
    drv_param_init.o(i.drv_param_init_set_ccm) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_set_scld_filter) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_set_sclu_filter) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_p2r_filter_init) refers to drv_param_init.o(.constdata) for .constdata
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_dma.o(i.drv_dma_disenable_channel_interrupts) for drv_dma_disenable_channel_interrupts
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_master.o(i.drv_spi_m_enable_rx_dma) for drv_spi_m_enable_rx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_slave.o(i.drv_spi_s_enable_tx_dma) for drv_spi_s_enable_tx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_slave.o(i.drv_spi_s_enable_rx_dma) for drv_spi_s_enable_rx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_dma.o(i.drv_spi_dma_callback) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_dma_ch6_init) refers to drv_spi_dma.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_dma.o(i.drv_spi_dma_ch6_init) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_dma_init) refers to drv_spi_dma.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_dma.o(i.drv_spi_dma_init) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_spi_dma.o(i.drv_spi_dma_callback) for drv_spi_dma_callback
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_spi_dma.o(i.drv_spi_dma_callback) for drv_spi_dma_callback
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_spi_master.o(i.drv_spi_m_enable_rx_dma) for drv_spi_m_enable_rx_dma
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_spi_slave.o(i.drv_spi_s_enable_tx_dma) for drv_spi_s_enable_tx_dma
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_master.o(i.app_SPIM_IRQn_Handler) refers to drv_spi_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_master.o(i.app_SPIM_IRQn_Handler) refers to drv_spi_master.o(.data) for .data
    drv_spi_master.o(i.drv_spi_m_deinit) refers to drv_spi_master.o(i.drv_spi_m_switch_sclk) for drv_spi_m_switch_sclk
    drv_spi_master.o(i.drv_spi_m_disable_int) refers to drv_spi_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_master.o(i.drv_spi_m_set_intr_callback) refers to drv_spi_master.o(.data) for .data
    drv_spi_master.o(i.drv_spi_master_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_spi_master.o(i.drv_spi_master_init) refers to drv_common.o(.data) for g_system_clock
    drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig) for drv_sys_cfg_sel_ap_rst_lvl_trig
    drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect) refers to drv_sys_cfg.o(.data) for .data
    drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig) for drv_sys_cfg_sel_ap_rst_lvl_trig
    drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) refers to drv_sys_cfg.o(.data) for .data
    hal_internal_soft_sync.o(i.hal_intl_svs_deinit_rx) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_soft_sync.o(i.hal_intl_svs_deinit_rx) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.hal_intl_svs_deinit_rx) refers to hal_internal_soft_sync.o(i.svs_wait_start) for svs_wait_start
    hal_internal_soft_sync.o(i.hal_intl_svs_deinit_tx) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.hal_intl_svs_handle) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.hal_intl_svs_init_rx) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_soft_sync.o(i.hal_intl_svs_init_rx) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_soft_sync.o(i.hal_intl_svs_init_rx) refers to hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk) for hal_intl_svs_update_rxbr_clk
    hal_internal_soft_sync.o(i.hal_intl_svs_init_rx) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.hal_intl_svs_init_rx) refers to hal_internal_soft_sync.o(i.svs_wait_start) for svs_wait_start
    hal_internal_soft_sync.o(i.hal_intl_svs_init_tx) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.hal_intl_svs_set_input_frate) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_soft_sync.o(i.hal_intl_svs_set_input_frate) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_soft_sync.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_soft_sync.o(i.svs_wait_start) for svs_wait_start
    hal_internal_soft_sync.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_soft_sync.o(i.svs_waite_fr_stab) for svs_waite_fr_stab
    hal_internal_soft_sync.o(i.hal_intl_svs_set_sync_coef) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk) refers to dmul.o(.text) for __aeabi_dmul
    hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.svs_direct_mode_setting) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_soft_sync.o(i.svs_direct_mode_setting) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_internal_soft_sync.o(i.svs_direct_mode_setting) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_soft_sync.o(i.svs_direct_mode_setting) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg) for drv_rxbr_hline_rcv1_cfg
    hal_internal_soft_sync.o(i.svs_direct_mode_setting) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.svs_get_rel_intv) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_soft_sync.o(i.svs_get_rel_intv) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to hal_internal_soft_sync.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to f2d.o(.text) for __aeabi_f2d
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to dadd.o(.text) for __aeabi_dadd
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.svs_wait_start) refers to hal_internal_soft_sync.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_soft_sync.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_internal_soft_sync.o(i.svs_wait_start) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_soft_sync.o(i.svs_wait_start) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_soft_sync.o(i.svs_wait_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_internal_soft_sync.o(i.svs_wait_start) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_soft_sync.o(i.svs_wait_start) refers to f2d.o(.text) for __aeabi_f2d
    hal_internal_soft_sync.o(i.svs_wait_start) refers to ceil.o(i.ceil) for ceil
    hal_internal_soft_sync.o(i.svs_wait_start) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_soft_sync.o(i.svs_wait_start) refers to hal_internal_soft_sync.o(i.svs_direct_mode_setting) for svs_direct_mode_setting
    hal_internal_soft_sync.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg) for drv_rxbr_hline_rcv1_cfg
    hal_internal_soft_sync.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_soft_sync.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_soft_sync.o(i.svs_wait_start) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_soft_sync.o(i.svs_wait_start) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.svs_wait_start) refers to hal_internal_soft_sync.o(i.svs_waite_fr_stab) for svs_waite_fr_stab
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to hal_internal_soft_sync.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to ffixui.o(.text) for __aeabi_f2uiz
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to hal_internal_soft_sync.o(i.svs_sync_handle) for svs_sync_handle
    drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to ffltui.o(.text) for __aeabi_ui2f
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fdiv.o(.text) for __aeabi_fdiv
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fmul.o(.text) for __aeabi_fmul
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) for drv_dsi_rx_get_color_bpp
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc) for drv_dsi_rx_get_color_pcc
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fadd.o(.text) for __aeabi_fadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to cfrcmple.o(.text) for __aeabi_cfrcmple
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to f2d.o(.text) for __aeabi_f2d
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dadd.o(.text) for __aeabi_dadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dfixui.o(.text) for __aeabi_d2uiz
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte) for drv_rx_phy_test_write_1_byte
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to drv_dsi_rx.o(i.drv_rx_phy_test_read) for drv_rx_phy_test_read
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap) refers to drv_chip_info.o(i.drv_chip_info_get_info) for drv_chip_info_get_info
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_get_rate_para) for drv_phy_get_rate_para
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_get_calibration) for drv_phy_get_calibration
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_clear) for drv_rx_phy_test_clear
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte) for drv_rx_phy_test_write_1_byte
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte) for drv_rx_phy_test_write_2_byte
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_chip_info.o(i.drv_chip_info_get_info) for drv_chip_info_get_info
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_lock) for drv_rx_phy_test_lock
    drv_dsi_rx.o(i.drv_rx_phy_test_clear) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_rx.o(i.drv_rx_phy_test_lock) refers to drv_phy_common.o(i.drv_phy_test_lock) for drv_phy_test_lock
    drv_dsi_rx.o(i.drv_rx_phy_test_read) refers to drv_phy_common.o(i.drv_phy_test_read) for drv_phy_test_read
    drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_1_byte) for drv_phy_test_write_1_byte
    drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_2_byte) for drv_phy_test_write_2_byte
    drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) for drv_tx_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to drv_dsi_tx.o(i.drv_tx_phy_test_read) for drv_tx_phy_test_read
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_get_rate_para) for drv_phy_get_rate_para
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_get_pll_para) for drv_phy_get_pll_para
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_get_calibration) for drv_phy_get_calibration
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_enter) for drv_tx_phy_test_enter
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_crgu.o(i.drv_crgu_set_mipi_ref_src) for drv_crgu_set_mipi_ref_src
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_crgu.o(i.drv_crgu_set_mipi_cfg_src) for drv_crgu_set_mipi_cfg_src
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_clear) for drv_tx_phy_test_clear
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) for drv_tx_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte) for drv_tx_phy_test_write_2_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_code) for drv_tx_phy_test_write_code
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_exit) for drv_tx_phy_test_exit
    drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) for drv_tx_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_version) for drv_dsi_tx_version
    drv_dsi_tx.o(i.drv_dsi_tx_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_tx.o(i.drv_dsi_tx_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dsi_tx.o(i.drv_tx_phy_test_clear) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_tx.o(i.drv_tx_phy_test_read) refers to drv_phy_common.o(i.drv_phy_test_read) for drv_phy_test_read
    drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_1_byte) for drv_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_2_byte) for drv_phy_test_write_2_byte
    drv_dsi_tx.o(i.drv_tx_phy_test_write_code) refers to drv_phy_common.o(i.drv_phy_test_write_code) for drv_phy_test_write_code
    drv_lcdc.o(i.drv_lcdc_config_src_parameter) refers to drv_lcdc.o(i.drv_lcdc_config_input_size) for drv_lcdc_config_input_size
    drv_lcdc.o(i.drv_lcdc_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_lcdc.o(i.drv_lcdc_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_memc.o(i.app_MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_get_status) for drv_memc_get_status
    drv_memc.o(i.app_MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_clear_status) for drv_memc_clear_status
    drv_memc.o(i.app_MEMC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_rxbr.o(i.app_ADC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.app_ADC_IRQn_Handler) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.app_VPRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.app_VPRE_IRQn_Handler) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_EnableIRQ) for __NVIC_EnableIRQ
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_rxbr.o(i.drv_rxbr_register_irq0_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_register_irq1_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_set_cmd_filter) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_rxbr.o(i.drv_rxbr_soft_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_vidc.o(i.app_VIDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.app_VIDC_IRQn_Handler) refers to drv_vidc.o(.data) for .data
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_vidc.o(i.drv_vidc_register_callback) refers to drv_vidc.o(.data) for .data
    irq_redirect .o(i.ADC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.AP_NRESET_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.DMA_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT0_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT1_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT2_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT3_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT4_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT5_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT6_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT7_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.FLSCTRL_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.HardFault_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.I2C0_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.I2C1_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.LCDC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.MEMC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.MIPI_RX_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.MIPI_TX_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.PWMDET_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SPIM_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SPIS_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SWIRE_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SysTick_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER0_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER1_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER2_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER3_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.UART_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.VIDC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.VPRE_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.WDG_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.handle_init) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.handle_init) refers to drv_common.o(i.app_SysTick_Handler) for app_SysTick_Handler
    irq_redirect .o(i.handle_init) refers to hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) for app_LCDC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler) for app_MIPI_RX_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler) for app_MIPI_TX_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_dma.o(i.app_dma_irq_handler) for app_dma_irq_handler
    irq_redirect .o(i.handle_init) refers to norflash.o(i.app_fls_ctrl_Handler) for app_fls_ctrl_Handler
    irq_redirect .o(i.handle_init) refers to drv_i2c_slave.o(i.app_I2C0_IRQn_Handler) for app_I2C0_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_i2c_master.o(i.app_I2C1_IRQn_Handler) for app_I2C1_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to hal_spi_slave.o(i.app_SPIS_IRQn_Handler) for app_SPIS_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_spi_master.o(i.app_SPIM_IRQn_Handler) for app_SPIM_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_rxbr.o(i.app_VPRE_IRQn_Handler) for app_VPRE_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_rxbr.o(i.app_ADC_IRQn_Handler) for app_ADC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_vidc.o(i.app_VIDC_IRQn_Handler) for app_VIDC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_memc.o(i.app_MEMC_IRQn_Handler) for app_MEMC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER0_IRQn_Handler) for app_TIMER0_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER1_IRQn_Handler) for app_TIMER1_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER2_IRQn_Handler) for app_TIMER2_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER3_IRQn_Handler) for app_TIMER3_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_wdg.o(i.app_WDG_IRQn_Handler) for app_WDG_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_uart.o(i.app_UART_IRQn_Handler) for app_UART_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_pwm.o(i.app_PWMDET_IRQn_Handler) for app_PWMDET_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_swire.o(i.app_SWIRE_IRQn_Handler) for app_SWIRE_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) for app_AP_NRESET_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler) for app_EXTI_INT0_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler) for app_EXTI_INT1_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler) for app_EXTI_INT2_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler) for app_EXTI_INT3_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler) for app_EXTI_INT4_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler) for app_EXTI_INT5_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler) for app_EXTI_INT6_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler) for app_EXTI_INT7_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_common.o(i.app_HardFault_Handler) for app_HardFault_Handler
    drv_efuse.o(i.drv_efuse_enter_inactive) refers to drv_efuse.o(i.drv_efuse_int_enable) for drv_efuse_int_enable
    drv_efuse.o(i.drv_efuse_read) refers to drv_efuse.o(i.drv_efuse_read_req) for drv_efuse_read_req
    drv_efuse.o(i.drv_efuse_write) refers to drv_efuse.o(i.drv_efuse_write_req) for drv_efuse_write_req
    drv_phy_common.o(i.drv_phy_enable_calibration) refers to drv_phy_common.o(.data) for .data
    drv_phy_common.o(i.drv_phy_get_calibration) refers to drv_chip_info.o(i.drv_chip_info_get_info) for drv_chip_info_get_info
    drv_phy_common.o(i.drv_phy_get_calibration) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_phy_common.o(i.drv_phy_get_calibration) refers to drv_phy_common.o(.data) for .data
    drv_phy_common.o(i.drv_phy_get_pll_para) refers to drv_phy_common.o(.constdata) for .constdata
    drv_phy_common.o(i.drv_phy_get_rate_para) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_phy_common.o(i.drv_phy_get_rate_para) refers to drv_phy_common.o(.constdata) for .constdata
    drv_phy_common.o(i.drv_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_code) for drv_phy_test_write_code
    drv_phy_common.o(i.drv_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_data) for drv_phy_test_write_data
    drv_phy_common.o(i.drv_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_code) for drv_phy_test_write_code
    drv_phy_common.o(i.drv_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_data) for drv_phy_test_write_data
    drv_chip_info.o(i.drv_chip_info_get_info) refers to drv_chip_info.o(.data) for .data
    drv_chip_info.o(i.drv_chip_info_init) refers to drv_efuse.o(i.drv_efuse_enter_inactive) for drv_efuse_enter_inactive
    drv_chip_info.o(i.drv_chip_info_init) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_chip_info.o(i.drv_chip_info_init) refers to drv_chip_info.o(.data) for .data
    drv_chip_info.o(i.drv_chip_rx_info_check) refers to printfa.o(i.__0printf) for __2printf
    drv_chip_info.o(i.drv_chip_rx_info_check) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_chip_info.o(i.drv_chip_rx_info_check) refers to drv_chip_info.o(.data) for .data
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to drv_efuse.o(i.drv_efuse_enter_inactive) for drv_efuse_enter_inactive
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to printfa.o(i.__0printf) for __2printf
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to hal_spi_slave.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_spi_slave.o(i.hal_spi_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    hal_spi_slave.o(i.hal_spi_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_abort) refers to drv_spi_dma.o(i.drv_spi_abort_dma) for drv_spi_abort_dma
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start) refers to drv_dma.o(i.drv_dma_enable_cycle) for drv_dma_enable_cycle
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start) refers to drv_spi_dma.o(i.drv_spis_dma_write) for drv_spis_dma_write
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_deinit) refers to drv_spi_slave.o(i.drv_spi_s_deinit) for drv_spi_s_deinit
    hal_spi_slave.o(i.hal_spi_slave_enable) refers to drv_spi_slave.o(i.drv_spi_s_enable_int) for drv_spi_s_enable_int
    hal_spi_slave.o(i.hal_spi_slave_enable) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_spi_slave.o(i.hal_spi_slave_enable) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_gpio_init) refers to drv_spi_slave.o(i.drv_spi_s_gpio_init) for drv_spi_s_gpio_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to hal_spi_slave.o(i.hal_spi_slave_gpio_init) for hal_spi_slave_gpio_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_slave.o(i.drv_spi_slave_init) for drv_spi_slave_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_dma.o(i.drv_spi_dma_init) for drv_spi_dma_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) for drv_spi_set_dma_irq_callback
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_slave.o(i.drv_spi_s_enable_tx_dma) for drv_spi_s_enable_tx_dma
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    hal_spi_slave.o(i.hal_spi_slave_init) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_read_data) refers to drv_spi_slave.o(i.drv_spi_s_read_data) for drv_spi_s_read_data
    hal_spi_slave.o(i.hal_spi_slave_register_callback) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_reset_tx) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_set_auto_rx_buffer) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_set_auto_tx_buffer) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_write_data) refers to drv_spi_slave.o(i.drv_spi_s_write_data) for drv_spi_s_write_data
    norflash.o(i.app_fls_ctrl_Handler) refers to drv_fls.o(i.fls_clr_interrupt_flag) for fls_clr_interrupt_flag
    norflash.o(i.app_fls_ctrl_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    norflash.o(i.app_fls_ctrl_Handler) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_best_cfg_init) refers to drv_fls.o(i.fls_spi_init) for fls_spi_init
    norflash.o(i.norflash_best_cfg_init) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_check_id) refers to norflash.o(i.norflash_read_id) for norflash_read_id
    norflash.o(i.norflash_check_id) refers to tau_delay.o(i.delayUs) for delayUs
    norflash.o(i.norflash_check_id) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dma_callback) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dma_read) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_transfer_create_handle_dma) for fls_transfer_create_handle_dma
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_dma_read_prepare) for fls_dma_read_prepare
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_transfer_dma) for fls_transfer_dma
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    norflash.o(i.norflash_dma_read) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dma_read) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_dma_read) refers to norflash.o(i.norflash_dma_callback) for norflash_dma_callback
    norflash.o(i.norflash_dma_write) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_transfer_create_handle_dma) for fls_transfer_create_handle_dma
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_switch_fls_spi) for norflash_switch_fls_spi
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_dma_write_prepare) for fls_dma_write_prepare
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_transfer_dma) for fls_transfer_dma
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    norflash.o(i.norflash_dma_write) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_dma_write) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_dma_callback) for norflash_dma_callback
    norflash.o(i.norflash_dma_write) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dual_read) refers to drv_fls.o(i.fls_ddat_enable) for fls_ddat_enable
    norflash.o(i.norflash_dual_read) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_dual_read) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_switch_fls_spi) for norflash_switch_fls_spi
    norflash.o(i.norflash_dual_write) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_dual_write) refers to drv_fls.o(i.fls_ddat_enable) for fls_ddat_enable
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_en4b) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_read_config_reg) for norflash_read_config_reg
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_en_quad) refers to norflash.o(i.norflash_en_quad_check) for norflash_en_quad_check
    norflash.o(i.norflash_en_quad) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_en_quad) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_en_quad) refers to drv_fls.o(i.fls_busy_pending) for fls_busy_pending
    norflash.o(i.norflash_en_quad) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(i.norflash_get_dual_hstatus) for norflash_get_dual_hstatus
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(i.norflash_get_hstatus) for norflash_get_hstatus
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_erase_block) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_erase_block) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_erase_block) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_erase_block) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_erase_chip) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_erase_chip) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_erase_chip) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_erase_sector) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_erase_sector) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_erase_sector) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_erase_sector) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_ex4b) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_read_config_reg) for norflash_read_config_reg
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_exit_quad) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_exit_quad) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_exit_quad) refers to norflash.o(i.norflash_en_quad_check) for norflash_en_quad_check
    norflash.o(i.norflash_exit_quad) refers to drv_fls.o(i.fls_busy_pending) for fls_busy_pending
    norflash.o(i.norflash_exit_quad) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_get_dual_hstatus) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_get_dual_hstatus) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_get_dual_hstatus) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_get_hstatus) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_get_hstatus) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_get_hstatus) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_get_status) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_get_status) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_get_status) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_get_default_spi_config) for fls_get_default_spi_config
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_get_default_fls_config) for fls_get_default_fls_config
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_get_default_tuning) for fls_get_default_tuning
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_init) for fls_init
    norflash.o(i.norflash_init) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_init) refers to drv_fls.o(.data) for g_fls_tuning
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_qdat_enable) for fls_qdat_enable
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_qadr_enable) for fls_qadr_enable
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_qcmd_enable) for fls_qcmd_enable
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_switch_fls_spi) for norflash_switch_fls_spi
    norflash.o(i.norflash_quad_write) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_quad_write) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_read) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_read_config_reg) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_read_id) refers to drv_fls.o(i.fls_read_cmd) for fls_read_cmd
    norflash.o(i.norflash_read_uid) refers to memseta.o(.text) for __aeabi_memclr4
    norflash.o(i.norflash_read_uid) refers to drv_fls.o(i.fls_read_cmd) for fls_read_cmd
    norflash.o(i.norflash_read_uid) refers to memcpya.o(.text) for __aeabi_memcpy
    norflash.o(i.norflash_set_best_cfg) refers to memseta.o(.text) for __aeabi_memclr4
    norflash.o(i.norflash_set_best_read_cfg) refers to norflash.o(i.norflash_en_quad) for norflash_en_quad
    norflash.o(i.norflash_set_best_read_cfg) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_set_best_read_cfg) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_set_best_write_cfg) refers to norflash.o(i.norflash_en_quad) for norflash_en_quad
    norflash.o(i.norflash_set_best_write_cfg) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_set_best_write_cfg) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_ddat_enable) for fls_ddat_enable
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_qdat_enable) for fls_qdat_enable
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_qadr_enable) for fls_qadr_enable
    norflash.o(i.norflash_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_write) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_write_disable) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_write_disable) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write_disable) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_write_disable) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_write_enable) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_write_enable) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write_enable) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_write_enable) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_big_end_enable) for norflash_big_end_enable
    norflash.o(i.norflash_write_endian_scr) refers to drv_fls.o(i.fls_en_scr) for fls_en_scr
    norflash.o(i.norflash_write_endian_scr) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_big_end_clear) for norflash_big_end_clear
    norflash.o(i.norflash_write_endian_scr) refers to drv_fls.o(i.fls_scr_clear) for fls_scr_clear
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    drv_fls_dma.o(i.fls_abort_dma) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_fls_dma.o(i.fls_abort_dma) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls_dma.o(i.fls_dma_enable) for fls_dma_enable
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_set_write) for fls_set_write
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls_dma.o(i.fls_dma_enable) for fls_dma_enable
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls_dma.o(i.fls_read_dmacallback) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to memseta.o(.text) for __aeabi_memclr4
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_fls_dma.o(.data) for .data
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_fls_dma.o(i.fls_read_dmacallback) for fls_read_dmacallback
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_fls_dma.o(i.fls_write_dmacallback) for fls_write_dmacallback
    drv_fls_dma.o(i.fls_transfer_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_fls_dma.o(i.fls_transfer_dma) refers to drv_dma.o(i.drv_dma_start_transfer) for drv_dma_start_transfer
    drv_fls_dma.o(i.fls_transfer_get_receive_count_dma) refers to drv_dma.o(i.drv_dma_get_remaining_bytes) for drv_dma_get_remaining_bytes
    drv_fls_dma.o(i.fls_write_dmacallback) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_pwm.o(i.app_PWMDET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_pwm.o(i.app_PWMDET_IRQn_Handler) refers to drv_pwm.o(.data) for .data
    drv_pwm.o(i.drv_pwm_in_register_callback) refers to drv_pwm.o(.data) for .data
    drv_pwm.o(i.drv_pwm_in_set_sys_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_pwm.o(i.drv_pwm_in_set_sys_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_spi_slave.o(i.drv_spi_s_deinit) refers to drv_spi_slave.o(i.drv_spi_s_switch_sclk) for drv_spi_s_switch_sclk
    drv_swire.o(i.app_SWIRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_swire.o(i.app_SWIRE_IRQn_Handler) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    drv_swire.o(i.app_SWIRE_IRQn_Handler) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_register_callback) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_swire.o(i.drv_swire_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_timer.o(i.app_TIMER0_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.app_TIMER1_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.app_TIMER2_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.app_TIMER3_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_timer.o(i.drv_timer_enable) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_get_instance) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_get_prescaler) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_get_status) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_clear_status_flags) for drv_timer_clear_status_flags
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_register_callback) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_compare_val) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_timer.o(i.drv_timer_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_repeat) refers to drv_timer.o(.data) for .data
    drv_uart.o(i.UART0_IRQ_Handle) refers to drv_uart.o(i.UART_TransferHandleIRQ) for UART_TransferHandleIRQ
    drv_uart.o(i.UART0_IRQ_Handle) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_uart.o(i.UART0_IRQ_Handle) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_AbortReceive) refers to drv_uart.o(i.UART_Disable_IT) for UART_Disable_IT
    drv_uart.o(i.UART_AbortReceive) refers to drv_uart.o(i.UART_ResetRxFIFO) for UART_ResetRxFIFO
    drv_uart.o(i.UART_AbortSend) refers to drv_uart.o(i.UART_Disable_IT) for UART_Disable_IT
    drv_uart.o(i.UART_AbortSend) refers to drv_uart.o(i.UART_ResetTxFIFO) for UART_ResetTxFIFO
    drv_uart.o(i.UART_Deinit) refers to drv_uart.o(i.UART_SwitchSCLK) for UART_SwitchSCLK
    drv_uart.o(i.UART_Disable_IT) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_Disable_IT) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.UART_Disable_IT) refers to drv_uart.o(.constdata) for .constdata
    drv_uart.o(i.UART_EnableDma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req) for drv_sys_cfg_set_dma_rx_req
    drv_uart.o(i.UART_EnableDma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    drv_uart.o(i.UART_Enable_IT) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_Enable_IT) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.UART_GetDefaultConfig) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.UART_GetDefaultConfig) refers to drv_common.o(.data) for g_system_clock
    drv_uart.o(i.UART_GetFIFO_Ctrl) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_GetFIFO_Ctrl) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_ResetRxFIFO) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_ResetRxFIFO) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_ResetTxFIFO) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_ResetTxFIFO) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_SetBaudRate) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_uart.o(i.UART_SwitchSCLK) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_uart.o(i.UART_TransferCreateHandle) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_TransferCreateHandle) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.UART_TransferCreateHandle) refers to drv_uart.o(i.UART_Enable_IT) for UART_Enable_IT
    drv_uart.o(i.UART_TransferCreateHandle) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_TransferHandleIRQ) refers to drv_uart.o(i.UART_ResetRxFIFO) for UART_ResetRxFIFO
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_DisableDma) for UART_DisableDma
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_SwitchSCLK) for UART_SwitchSCLK
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_SetBaudRate) for UART_SetBaudRate
    drv_uart.o(i.UART_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.UART_init) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.app_UART_IRQn_Handler) refers to drv_uart.o(i.UART0_IRQ_Handle) for UART0_IRQ_Handle
    drv_uart_dma.o(i.UART_DMAInit) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart_dma.o(i.UART_DMAInit) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    drv_uart_dma.o(i.UART_TransferAbortReceiveDMA) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_uart_dma.o(i.UART_TransferAbortSendDMA) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart.o(i.UART_EnableDma) for UART_EnableDma
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(i.UART_DMAInit) for UART_DMAInit
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(.data) for .data
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(i.UART_TransferReceiveDMACallback) for UART_TransferReceiveDMACallback
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(i.UART_TransferSendDMACallback) for UART_TransferSendDMACallback
    drv_uart_dma.o(i.UART_TransferGetReceiveCountDMA) refers to drv_dma.o(i.drv_dma_get_remaining_bytes) for drv_dma_get_remaining_bytes
    drv_uart_dma.o(i.UART_TransferReceiveDMA) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_uart_dma.o(i.UART_TransferReceiveDMA) refers to drv_uart.o(i.UART_EnableDma) for UART_EnableDma
    drv_uart_dma.o(i.UART_TransferReceiveDMA) refers to drv_dma.o(i.drv_dma_start_transfer) for drv_dma_start_transfer
    drv_uart_dma.o(i.UART_TransferSendDMA) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_uart_dma.o(i.UART_TransferSendDMA) refers to drv_uart.o(i.UART_EnableDma) for UART_EnableDma
    drv_uart_dma.o(i.UART_TransferSendDMA) refers to drv_dma.o(i.drv_dma_start_transfer) for drv_dma_start_transfer
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_set_int) for drv_wdg_set_int
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_clear_counter) for drv_wdg_clear_counter
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_read_edge_flag) for drv_wdg_read_edge_flag
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_clear_edge_flag) for drv_wdg_clear_edge_flag
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(.data) for .data
    drv_wdg.o(i.drv_wdg_register_callback) refers to drv_wdg.o(.data) for .data
    drv_wdg.o(i.drv_wdg_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_wdg.o(i.drv_wdg_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_wdg.o(i.drv_wdg_set_repeat) refers to drv_wdg.o(.data) for .data
    dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_fifo_init) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_size) refers to dcs_packet_fifo.o(.bss) for .bss
    ceil.o(i.__softfp_ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.__softfp_ceil) refers to ceil.o(i.ceil) for ceil
    ceil.o(i.ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.ceil) refers to dadd.o(.text) for __aeabi_dadd
    ceil.o(i.ceil) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    sqrt.o(i.__softfp_sqrt) refers (Special) to iusefp.o(.text) for __I$use$fp
    sqrt.o(i.__softfp_sqrt) refers to dsqrt.o(.text) for _dsqrt
    sqrt.o(i.__softfp_sqrt) refers to errno.o(i.__set_errno) for __set_errno
    sqrt.o(i.sqrt) refers (Special) to iusefp.o(.text) for __I$use$fp
    sqrt.o(i.sqrt) refers to dsqrt.o(.text) for _dsqrt
    sqrt.o(i.sqrt) refers to errno.o(i.__set_errno) for __set_errno
    sqrt_x.o(i.____softfp_sqrt$lsc) refers (Special) to iusefp.o(.text) for __I$use$fp
    sqrt_x.o(i.____softfp_sqrt$lsc) refers to cdcmple.o(.text) for __aeabi_cdcmple
    sqrt_x.o(i.____softfp_sqrt$lsc) refers to errno.o(i.__set_errno) for __set_errno
    sqrt_x.o(i.____softfp_sqrt$lsc) refers to dsqrt.o(.text) for _dsqrt
    sqrt_x.o(i.__sqrt$lsc) refers (Special) to iusefp.o(.text) for __I$use$fp
    sqrt_x.o(i.__sqrt$lsc) refers to cdcmple.o(.text) for __aeabi_cdcmple
    sqrt_x.o(i.__sqrt$lsc) refers to errno.o(i.__set_errno) for __set_errno
    sqrt_x.o(i.__sqrt$lsc) refers to dsqrt.o(.text) for _dsqrt
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry10a.o(.ARM.Collect$$$$0000000D) for __rt_final_cpp
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry11a.o(.ARM.Collect$$$$0000000F) for __rt_final_exit
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry7b.o(.ARM.Collect$$$$00000008) for _main_clock
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry8b.o(.ARM.Collect$$$$0000000A) for _main_cpp_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry9a.o(.ARM.Collect$$$$0000000B) for _main_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry5.o(.ARM.Collect$$$$00000004) for _main_scatterload
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry2.o(.ARM.Collect$$$$00000001) for _main_stk
    idiv.o(.text) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfb.o(i.__0fprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0fprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0printf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printfb.o(i.__0vfprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vfprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printf0.o(i.__0fprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0fprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0printf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf0.o(i.__0vfprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vfprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf1.o(i.__0fprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0fprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0printf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i.__0vfprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vfprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf2.o(i.__0fprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0fprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0printf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf2.o(i.__0vfprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vfprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf3.o(i.__0fprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0fprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0printf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i.__0vfprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vfprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf4.o(i.__0fprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0fprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0printf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i.__0vfprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vfprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf5.o(i.__0fprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0fprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0printf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i.__0vfprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vfprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf6.o(i.__0fprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0fprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0printf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i.__0vfprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vfprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i._printf_core) refers to printf6.o(i._printf_pre_padding) for _printf_pre_padding
    printf6.o(i._printf_core) refers to printf6.o(i._printf_post_padding) for _printf_post_padding
    printf6.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf7.o(i.__0fprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0fprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0printf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i.__0vfprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vfprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i._printf_core) refers to printf7.o(i._printf_pre_padding) for _printf_pre_padding
    printf7.o(i._printf_core) refers to printf7.o(i._printf_post_padding) for _printf_post_padding
    printf7.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf8.o(i.__0fprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0fprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0printf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i.__0vfprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vfprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i._printf_core) refers to printf8.o(i._printf_pre_padding) for _printf_pre_padding
    printf8.o(i._printf_core) refers to printf8.o(i._printf_post_padding) for _printf_post_padding
    printf8.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i.__0fprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0fprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0fprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0printf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0printf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0snprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0snprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0snprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0sprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0sprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0sprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i.__0vfprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vfprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vfprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0vsnprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0vsprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i._fp_digits) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._fp_digits) refers to dmul.o(.text) for __aeabi_dmul
    printfa.o(i._fp_digits) refers to ddiv.o(.text) for __aeabi_ddiv
    printfa.o(i._fp_digits) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    printfa.o(i._fp_digits) refers to dadd.o(.text) for __aeabi_dadd
    printfa.o(i._fp_digits) refers to dfixul.o(.text) for __aeabi_d2ulz
    printfa.o(i._fp_digits) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_core) refers to printfa.o(i._printf_pre_padding) for _printf_pre_padding
    printfa.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers to printfa.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i._printf_core) refers to printfa.o(i._fp_digits) for _fp_digits
    printfa.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfa.o(i._printf_post_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_pre_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._snputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._sputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    fmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers to fepilogue.o(.text) for _float_round
    fscalb.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    dadd.o(.text) refers to llsshr.o(.text) for __aeabi_lasr
    dadd.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dmul.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ddiv.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ddiv.o(.text) refers to depilogue.o(.text) for _double_round
    fflti.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fflti.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    ffltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ffltui.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    dflti.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dflti.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dfltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfltui.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ffixi.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ffixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixi.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixi.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixui.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    f2d.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    cdcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    cfcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    cfrcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    entry2.o(.ARM.Collect$$$$00000001) refers to entry2.o(.ARM.Collect$$$$00002712) for __lit__00000000
    entry2.o(.ARM.Collect$$$$00002712) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    entry5.o(.ARM.Collect$$$$00000004) refers to init.o(.text) for __scatterload
    entry9a.o(.ARM.Collect$$$$0000000B) refers to main.o(i.main) for main
    entry9b.o(.ARM.Collect$$$$0000000C) refers to main.o(i.main) for main
    uldiv.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    uldiv.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    errno.o(i.__aeabi_errno_addr) refers to errno.o(.data) for .data
    errno.o(i.__read_errno) refers to errno.o(.data) for .data
    errno.o(i.__set_errno) refers to errno.o(.data) for .data
    depilogue.o(.text) refers to depilogue.o(i.__ARM_clz) for __ARM_clz
    depilogue.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dsqrt.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dsqrt.o(.text) refers to depilogue.o(.text) for _double_round
    dfixul.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixul.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    init.o(.text) refers to entry5.o(.ARM.Collect$$$$00000004) for __main_after_scatterload


==============================================================================

Removing Unused input sections from the image.

    Removing main.o(.rev16_text), (4 bytes).
    Removing main.o(.revsh_text), (4 bytes).
    Removing ap_demo.o(.rev16_text), (4 bytes).
    Removing ap_demo.o(.revsh_text), (4 bytes).
    Removing ap_demo.o(i.tp_heartbeat_exec), (104 bytes).
    Removing ap_demo.o(i.tp_power_up_restart), (36 bytes).
    Removing ap_demo.o(.data), (1 bytes).
    Removing ap_demo.o(.data), (2 bytes).
    Removing ap_demo.o(.data), (1 bytes).
    Removing ap_demo.o(.data), (256 bytes).
    Removing ap_demo.o(.data), (256 bytes).
    Removing ap_demo.o(.data), (2 bytes).
    Removing ap_demo.o(.data), (2 bytes).
    Removing ap_demo.o(.data), (2 bytes).
    Removing ap_demo.o(.data), (2 bytes).
    Removing app_tp_transfer.o(.rev16_text), (4 bytes).
    Removing app_tp_transfer.o(.revsh_text), (4 bytes).
    Removing app_tp_transfer.o(i.S20_Start_init), (356 bytes).
    Removing app_tp_transfer.o(i.app_tp_I2C_init), (36 bytes).
    Removing app_tp_transfer.o(i.app_tp_i2cs_callback), (64 bytes).
    Removing app_tp_transfer.o(i.app_tp_init), (64 bytes).
    Removing app_tp_transfer.o(i.app_tp_m_read), (32 bytes).
    Removing app_tp_transfer.o(i.app_tp_m_transfer_complate), (8 bytes).
    Removing app_tp_transfer.o(i.app_tp_m_write), (8 bytes).
    Removing app_tp_transfer.o(i.app_tp_phone_clear_reset_on), (12 bytes).
    Removing app_tp_transfer.o(i.app_tp_phone_reset_on), (12 bytes).
    Removing app_tp_transfer.o(i.app_tp_s_read), (8 bytes).
    Removing app_tp_transfer.o(i.app_tp_s_transfer_complate), (26 bytes).
    Removing app_tp_transfer.o(i.app_tp_s_write), (8 bytes).
    Removing app_tp_transfer.o(i.app_tp_screen_init), (48 bytes).
    Removing app_tp_transfer.o(i.app_tp_screen_int_callback), (12 bytes).
    Removing app_tp_transfer.o(i.app_tp_transfer_screen_const), (64 bytes).
    Removing app_tp_transfer.o(i.app_tp_transfer_screen_int), (276 bytes).
    Removing app_tp_transfer.o(i.app_tp_transfer_screen_start), (24 bytes).
    Removing app_tp_transfer.o(.bss), (400 bytes).
    Removing app_tp_transfer.o(.data), (23 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (5 bytes).
    Removing app_tp_transfer.o(.data), (6 bytes).
    Removing app_tp_transfer.o(.data), (2 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (4 bytes).
    Removing app_tp_transfer.o(.data), (4 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (1 bytes).
    Removing app_tp_transfer.o(.data), (2 bytes).
    Removing app_tp_transfer.o(.data), (2 bytes).
    Removing app_tp_st_touch.o(.rev16_text), (4 bytes).
    Removing app_tp_st_touch.o(.revsh_text), (4 bytes).
    Removing app_tp_st_touch.o(i.CRC16_2), (64 bytes).
    Removing app_tp_st_touch.o(i.ap_set_tp_calibration_04), (152 bytes).
    Removing app_tp_st_touch.o(i.ap_tp_st_touch_calibration), (176 bytes).
    Removing app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_F3), (26 bytes).
    Removing app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_FF), (32 bytes).
    Removing app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark), (168 bytes).
    Removing app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset), (188 bytes).
    Removing app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init), (28 bytes).
    Removing app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event), (148 bytes).
    Removing app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec), (80 bytes).
    Removing app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event), (52 bytes).
    Removing app_tp_st_touch.o(i.ap_tp_st_touch_software_reset), (112 bytes).
    Removing app_tp_st_touch.o(i.app_tp_calibration_exec), (168 bytes).
    Removing app_tp_st_touch.o(i.app_tp_phone_analysis_data_for_wake_up), (64 bytes).
    Removing app_tp_st_touch.o(i.app_tp_screen_analysis_wake_up), (160 bytes).
    Removing app_tp_st_touch.o(i.app_tp_screen_analysis_wake_up_exec), (192 bytes).
    Removing app_tp_st_touch.o(.bss), (28 bytes).
    Removing app_tp_st_touch.o(.constdata), (32 bytes).
    Removing board.o(.rev16_text), (4 bytes).
    Removing board.o(.revsh_text), (4 bytes).
    Removing startup_armcm0.o(HEAP), (3072 bytes).
    Removing app_tp_for_custom_s8.o(.rev16_text), (4 bytes).
    Removing app_tp_for_custom_s8.o(.revsh_text), (4 bytes).
    Removing app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data), (852 bytes).
    Removing app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const), (56 bytes).
    Removing app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int), (684 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (5286 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (1120 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (1120 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (288 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (1 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (3 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (3 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (1 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (3 bytes).
    Removing app_tp_for_custom_s8.o(.data), (5 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (48 bytes).
    Removing app_tp_for_custom_s8.o(.data), (64 bytes).
    Removing app_tp_for_custom_s8.o(.data), (3 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (32 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing hal_dsi_rx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd), (88 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_short_cmd), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video), (228 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit), (176 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init), (48 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern), (216 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en), (16 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode), (100 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_write_cmd_entry), (10 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle), (40 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_dcs_direct_mode), (8 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter), (40 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode), (52 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format), (56 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data), (148 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data), (268 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk), (80 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode), (52 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_te_waveform), (52 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop), (60 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate), (10 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution_ex), (32 bytes).
    Removing hal_dsi_tx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic), (148 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode_rcv_te), (10 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit), (132 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard), (280 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker), (172 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_mode_init), (30 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_ulps_mode), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_ulps_mode), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd), (140 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle), (28 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_pq_filter), (28 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_lp_cmd), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data), (272 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg), (80 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop), (68 bytes).
    Removing hal_dsi_tx_ctrl.o(.constdata), (36 bytes).
    Removing hal_gpio.o(.rev16_text), (4 bytes).
    Removing hal_gpio.o(.revsh_text), (4 bytes).
    Removing hal_gpio.o(i.hal_gpio_ctrl_eint), (24 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_input_data), (18 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_int_type), (20 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_pull_state), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_init_eint), (64 bytes).
    Removing hal_gpio.o(i.hal_gpio_init_input), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_reg_eint_cb), (24 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_ap_reset_int), (80 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_driving_strength), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_output_data_ex), (36 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_pull_state), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_schmitt_trigger), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_slew_rate), (32 bytes).
    Removing hal_i2c_master.o(.rev16_text), (4 bytes).
    Removing hal_i2c_master.o(.revsh_text), (4 bytes).
    Removing hal_i2c_master.o(i.hal_i2c_m_deinit), (8 bytes).
    Removing hal_i2c_master.o(i.hal_i2c_m_dma_init), (108 bytes).
    Removing hal_i2c_master.o(i.hal_i2c_m_dma_read), (32 bytes).
    Removing hal_i2c_master.o(i.hal_i2c_m_dma_write), (28 bytes).
    Removing hal_i2c_master.o(i.hal_i2c_m_set_high_impedance), (46 bytes).
    Removing hal_i2c_master.o(i.hal_i2c_m_transfer_complate), (12 bytes).
    Removing hal_i2c_master.o(i.hal_i2c_master_irq_callback), (32 bytes).
    Removing hal_i2c_master.o(.data), (1 bytes).
    Removing hal_i2c_slave.o(.rev16_text), (4 bytes).
    Removing hal_i2c_slave.o(.revsh_text), (4 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_deinit), (88 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback), (16 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_dma_write), (76 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_get_tx_byte_num), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_init), (200 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read), (20 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_read_complate), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_read_complate_clear), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_read_data), (32 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_rxfifo_notempty), (40 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_sel), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_set_dma_tx_cycle), (36 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance), (88 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_set_transfer), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_write_complate), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_write_data), (32 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_slave_irq_callback), (372 bytes).
    Removing hal_i2c_slave.o(.constdata), (32 bytes).
    Removing hal_i2c_slave.o(.data), (32 bytes).
    Removing hal_spi_master.o(.rev16_text), (4 bytes).
    Removing hal_spi_master.o(.revsh_text), (4 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_callback), (24 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_clear_rxfifo), (14 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_deinit), (10 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_dma_init), (104 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_dma_read), (36 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_dma_write), (40 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_get_transfer_complate), (36 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_gpio_init), (8 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_read_rxfifo), (28 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_set_high_impedance), (100 bytes).
    Removing hal_spi_master.o(.data), (1 bytes).
    Removing hal_system.o(.rev16_text), (4 bytes).
    Removing hal_system.o(.revsh_text), (4 bytes).
    Removing hal_system.o(i.hal_system_clear_debug_state), (10 bytes).
    Removing hal_system.o(i.hal_system_deep_sleep_mode), (8 bytes).
    Removing hal_system.o(i.hal_system_disable_systick), (8 bytes).
    Removing hal_system.o(i.hal_system_get_debug_state), (8 bytes).
    Removing hal_system.o(i.hal_system_get_tick), (8 bytes).
    Removing hal_system.o(i.hal_system_idle_mode), (8 bytes).
    Removing hal_system.o(i.hal_system_register_systick_cb), (8 bytes).
    Removing hal_system.o(i.hal_system_reset_chip), (32 bytes).
    Removing hal_system.o(i.hal_system_set_pvd), (8 bytes).
    Removing hal_system.o(i.hal_system_set_vcc), (8 bytes).
    Removing hal_system.o(i.hal_system_share_flash_mode), (20 bytes).
    Removing hal_system.o(i.hal_system_sleep_mode), (48 bytes).
    Removing tau_delay.o(.rev16_text), (4 bytes).
    Removing tau_delay.o(.revsh_text), (4 bytes).
    Removing tau_log.o(.rev16_text), (4 bytes).
    Removing tau_log.o(.revsh_text), (4 bytes).
    Removing tau_log.o(i.fgetc), (22 bytes).
    Removing hal_uart.o(.rev16_text), (4 bytes).
    Removing hal_uart.o(.revsh_text), (4 bytes).
    Removing hal_uart.o(i.hal_uart_deinit), (28 bytes).
    Removing hal_uart.o(i.hal_uart_dmacallback), (36 bytes).
    Removing hal_uart.o(i.hal_uart_receive_blocking), (16 bytes).
    Removing hal_uart.o(i.hal_uart_receive_dma), (76 bytes).
    Removing hal_uart.o(i.hal_uart_transmit_dma), (76 bytes).
    Removing hal_internal_vsync.o(.rev16_text), (4 bytes).
    Removing hal_internal_vsync.o(.revsh_text), (4 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te), (168 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex), (468 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual), (512 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state), (12 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_register_write_cmd_entry), (12 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode), (48 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate), (152 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_update_lcdc_addr), (48 bytes).
    Removing hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler), (476 bytes).
    Removing drv_common.o(.rev16_text), (4 bytes).
    Removing drv_common.o(.revsh_text), (4 bytes).
    Removing drv_common.o(i.drv_common_disable_systick), (20 bytes).
    Removing drv_common.o(i.drv_common_get_tick), (12 bytes).
    Removing drv_common.o(i.drv_common_idle_mode), (40 bytes).
    Removing drv_common.o(i.drv_common_systick_register_cb), (12 bytes).
    Removing drv_crgu.o(.rev16_text), (4 bytes).
    Removing drv_crgu.o(.revsh_text), (4 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_all_reset_flags), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_reset_flag), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_config_clocks), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_config_clocks_div), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_config_clocks_src), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_ana_clk_status), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_clocks), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_fpga_id), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_mipi_ref_src), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_reset_flag), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_system_clk), (28 bytes).
    Removing drv_crgu.o(i.drv_crgu_reset_chip), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_200m_scan_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_300m_scan_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_abp0_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_adc_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_adc_src), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_apb1_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_apb2_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_fls_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_fls_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_monitor_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_monitor_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_swire_div), (20 bytes).
    Removing drv_dma.o(.rev16_text), (4 bytes).
    Removing drv_dma.o(.revsh_text), (4 bytes).
    Removing drv_dma.o(i.drv_dma_abort_transfer), (32 bytes).
    Removing drv_dma.o(i.drv_dma_ahb_init), (74 bytes).
    Removing drv_dma.o(i.drv_dma_channel_is_active), (20 bytes).
    Removing drv_dma.o(i.drv_dma_create_handle), (28 bytes).
    Removing drv_dma.o(i.drv_dma_deinit), (32 bytes).
    Removing drv_dma.o(i.drv_dma_disenable_channel), (16 bytes).
    Removing drv_dma.o(i.drv_dma_disenable_channel_interrupts), (24 bytes).
    Removing drv_dma.o(i.drv_dma_enable_channel), (16 bytes).
    Removing drv_dma.o(i.drv_dma_enable_channel_interrupts), (36 bytes).
    Removing drv_dma.o(i.drv_dma_enable_cycle), (44 bytes).
    Removing drv_dma.o(i.drv_dma_get_remaining_bytes), (32 bytes).
    Removing drv_dma.o(i.drv_dma_init), (24 bytes).
    Removing drv_dma.o(i.drv_dma_m2m_init), (72 bytes).
    Removing drv_dma.o(i.drv_dma_prepar_transfer), (18 bytes).
    Removing drv_dma.o(i.drv_dma_reset), (10 bytes).
    Removing drv_dma.o(i.drv_dma_set_burst), (26 bytes).
    Removing drv_dma.o(i.drv_dma_set_callback), (6 bytes).
    Removing drv_dma.o(i.drv_dma_set_ccr), (114 bytes).
    Removing drv_dma.o(i.drv_dma_set_transfer), (68 bytes).
    Removing drv_dma.o(i.drv_dma_start_transfer), (32 bytes).
    Removing drv_fls.o(.rev16_text), (4 bytes).
    Removing drv_fls.o(.revsh_text), (4 bytes).
    Removing drv_fls.o(i.__NVIC_DisableIRQ), (32 bytes).
    Removing drv_fls.o(i.drv_fls_gpio_connect), (28 bytes).
    Removing drv_fls.o(i.drv_fls_gpio_disconnect), (32 bytes).
    Removing drv_fls.o(i.fls_EnableClk), (12 bytes).
    Removing drv_fls.o(i.fls_busy_pending), (12 bytes).
    Removing drv_fls.o(i.fls_clear_irq_status), (6 bytes).
    Removing drv_fls.o(i.fls_ctrl_cfg_init), (72 bytes).
    Removing drv_fls.o(i.fls_ddat_enable), (24 bytes).
    Removing drv_fls.o(i.fls_de_init), (52 bytes).
    Removing drv_fls.o(i.fls_descr), (10 bytes).
    Removing drv_fls.o(i.fls_disable_it), (36 bytes).
    Removing drv_fls.o(i.fls_en_scr), (10 bytes).
    Removing drv_fls.o(i.fls_enable_it), (48 bytes).
    Removing drv_fls.o(i.fls_get_crcout), (4 bytes).
    Removing drv_fls.o(i.fls_get_default_fls_config), (20 bytes).
    Removing drv_fls.o(i.fls_get_default_spi_config), (44 bytes).
    Removing drv_fls.o(i.fls_get_default_tuning), (12 bytes).
    Removing drv_fls.o(i.fls_get_tuning), (18 bytes).
    Removing drv_fls.o(i.fls_init), (62 bytes).
    Removing drv_fls.o(i.fls_qadr_enable), (22 bytes).
    Removing drv_fls.o(i.fls_qcmd_enable), (22 bytes).
    Removing drv_fls.o(i.fls_qdat_enable), (22 bytes).
    Removing drv_fls.o(i.fls_read_byte_data), (130 bytes).
    Removing drv_fls.o(i.fls_read_cmd), (104 bytes).
    Removing drv_fls.o(i.fls_read_cmd_it), (110 bytes).
    Removing drv_fls.o(i.fls_reset_crc), (18 bytes).
    Removing drv_fls.o(i.fls_scr_clear), (10 bytes).
    Removing drv_fls.o(i.fls_set_addr_dummy), (32 bytes).
    Removing drv_fls.o(i.fls_set_addr_len), (32 bytes).
    Removing drv_fls.o(i.fls_set_mc_irq_mask), (26 bytes).
    Removing drv_fls.o(i.fls_set_read), (10 bytes).
    Removing drv_fls.o(i.fls_set_tuning), (24 bytes).
    Removing drv_fls.o(i.fls_set_write), (10 bytes).
    Removing drv_fls.o(i.fls_single_mode), (16 bytes).
    Removing drv_fls.o(i.fls_spi_init), (180 bytes).
    Removing drv_fls.o(i.fls_spi_start), (10 bytes).
    Removing drv_fls.o(i.fls_swrst), (18 bytes).
    Removing drv_fls.o(i.fls_write_byte_data), (164 bytes).
    Removing drv_fls.o(i.fls_write_cmd), (58 bytes).
    Removing drv_fls.o(.data), (4 bytes).
    Removing drv_gpio.o(.rev16_text), (4 bytes).
    Removing drv_gpio.o(.revsh_text), (4 bytes).
    Removing drv_gpio.o(i.drv_gpio_get_input_data), (24 bytes).
    Removing drv_gpio.o(i.drv_gpio_get_pull_state), (224 bytes).
    Removing drv_gpio.o(i.drv_gpio_register_ap_reset_callback), (12 bytes).
    Removing drv_gpio.o(i.drv_gpio_register_callback), (20 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_driving_strength), (312 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_int), (80 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_pull_state), (304 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_schmitt_trigger), (168 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_slew_rate), (168 bytes).
    Removing drv_i2c_dma.o(.rev16_text), (4 bytes).
    Removing drv_i2c_dma.o(.revsh_text), (4 bytes).
    Removing drv_i2c_dma.o(i.drv_i2c_dma_callback), (52 bytes).
    Removing drv_i2c_dma.o(i.drv_i2c_dma_init), (172 bytes).
    Removing drv_i2c_dma.o(i.drv_i2c_enable_rx_dma), (26 bytes).
    Removing drv_i2c_dma.o(i.drv_i2c_enable_tx_dma), (24 bytes).
    Removing drv_i2c_dma.o(i.drv_i2c_master_read_dma), (92 bytes).
    Removing drv_i2c_dma.o(i.drv_i2c_master_write_dma), (60 bytes).
    Removing drv_i2c_dma.o(i.drv_i2c_master_write_read_cmd), (62 bytes).
    Removing drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback), (88 bytes).
    Removing drv_i2c_dma.o(i.drv_i2c_slave_write_dma), (24 bytes).
    Removing drv_i2c_dma.o(.bss), (320 bytes).
    Removing drv_i2c_dma.o(.data), (8 bytes).
    Removing drv_i2c_master.o(.rev16_text), (4 bytes).
    Removing drv_i2c_master.o(.revsh_text), (4 bytes).
    Removing drv_i2c_master.o(i.__NVIC_ClearPendingIRQ), (24 bytes).
    Removing drv_i2c_master.o(i.drv_i2c1_set_callback), (12 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_bus_init), (36 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit), (96 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_deinit), (80 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_disable_intr), (16 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_enable), (16 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_enable_intr), (56 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_get_fifo_status), (28 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_read_data), (32 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_set_fifo_threshold), (24 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_set_sys_mask), (48 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_write_data), (32 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_master_init), (140 bytes).
    Removing drv_i2c_slave.o(.rev16_text), (4 bytes).
    Removing drv_i2c_slave.o(.revsh_text), (4 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c0_set_callback), (12 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit), (66 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_config_intr), (4 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_enable), (8 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status), (20 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_read_data), (30 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_set_fifo_threshold), (16 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_set_intr), (80 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_write_data), (28 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_slave_init), (50 bytes).
    Removing drv_param_init.o(.rev16_text), (4 bytes).
    Removing drv_param_init.o(.revsh_text), (4 bytes).
    Removing drv_param_init.o(i.drv_param_init_set_sclu_filter), (28 bytes).
    Removing drv_pwr.o(.rev16_text), (4 bytes).
    Removing drv_pwr.o(.revsh_text), (4 bytes).
    Removing drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_cp_mode), (32 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_frame_buff_pd), (28 bytes).
    Removing drv_spi_dma.o(.rev16_text), (4 bytes).
    Removing drv_spi_dma.o(.revsh_text), (4 bytes).
    Removing drv_spi_dma.o(i.__NVIC_ClearPendingIRQ), (24 bytes).
    Removing drv_spi_dma.o(i.drv_spi_abort_dma), (108 bytes).
    Removing drv_spi_dma.o(i.drv_spi_dma_callback), (60 bytes).
    Removing drv_spi_dma.o(i.drv_spi_dma_ch6_init), (208 bytes).
    Removing drv_spi_dma.o(i.drv_spi_dma_init), (220 bytes).
    Removing drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback), (48 bytes).
    Removing drv_spi_dma.o(i.drv_spi_set_dma_irq_callback), (88 bytes).
    Removing drv_spi_dma.o(i.drv_spim_dma_read), (96 bytes).
    Removing drv_spi_dma.o(i.drv_spim_dma_write), (60 bytes).
    Removing drv_spi_dma.o(i.drv_spis_dma_write), (72 bytes).
    Removing drv_spi_dma.o(.bss), (480 bytes).
    Removing drv_spi_dma.o(.data), (16 bytes).
    Removing drv_spi_master.o(.rev16_text), (4 bytes).
    Removing drv_spi_master.o(.revsh_text), (4 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_deinit), (40 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_disable_int), (68 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_enable_int), (72 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_enable_rx_dma), (32 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_enable_tx_dma), (28 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_get_dma_address), (8 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_gpio_init), (32 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_read_data), (32 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_set_intr_callback), (12 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_switch_sclk), (28 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_write_data), (44 bytes).
    Removing drv_spi_master.o(i.drv_spi_master_init), (164 bytes).
    Removing drv_sys_cfg.o(.rev16_text), (4 bytes).
    Removing drv_sys_cfg.o(.revsh_text), (4 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_dma_req_mask), (32 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_read_version0_id), (12 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig), (28 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group), (36 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig), (36 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_set_ap_reset), (28 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req), (16 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req), (16 bytes).
    Removing hal_internal_soft_sync.o(.rev16_text), (4 bytes).
    Removing hal_internal_soft_sync.o(.revsh_text), (4 bytes).
    Removing hal_internal_soft_sync.o(i.hal_intl_svs_deinit_rx), (48 bytes).
    Removing hal_internal_soft_sync.o(i.hal_intl_svs_set_input_frate), (120 bytes).
    Removing drv_dsi_rx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_rx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate), (66 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_version), (4 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration), (236 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg), (32 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg), (48 bytes).
    Removing drv_dsi_rx.o(i.drv_rx_phy_test_read), (12 bytes).
    Removing drv_dsi_tx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_tx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_force_interrupt), (8 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_get_phy_status), (6 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_forcepll), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration), (232 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_start), (18 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock), (10 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot), (62 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger), (92 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter), (344 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit), (276 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_sdf_3d), (28 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_bta), (22 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_vpg), (70 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_version), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_vid_shadow), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_read), (10 bytes).
    Removing drv_lcdc.o(.rev16_text), (4 bytes).
    Removing drv_lcdc.o(.revsh_text), (4 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_config_rgb_to_pentile), (6 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_enable), (42 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_update_shadow_reg), (12 bytes).
    Removing drv_memc.o(.rev16_text), (4 bytes).
    Removing drv_memc.o(.revsh_text), (4 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_frm_time), (14 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_int_frame), (28 bytes).
    Removing drv_memc.o(i.drv_memc_set_fb_remaining_line_trigger), (12 bytes).
    Removing drv_memc.o(i.drv_memc_set_read_trigger_line), (16 bytes).
    Removing drv_memc.o(i.drv_memc_set_te_ind), (16 bytes).
    Removing drv_memc.o(i.drv_memc_set_tear_hwclr), (16 bytes).
    Removing drv_memc.o(i.drv_memc_set_vidc_fb_arb), (14 bytes).
    Removing drv_memc.o(i.drv_memc_set_write_trigger_line), (16 bytes).
    Removing drv_rxbr.o(.rev16_text), (4 bytes).
    Removing drv_rxbr.o(.revsh_text), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_dsc_flush), (16 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_cur_hline_rcv_cnt), (8 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_ipi_vsync_interval), (8 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_pix_fmt), (8 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_cmd_filter), (204 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_col_addr), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_compress), (24 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_page_addr), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_soft_reset), (98 bytes).
    Removing drv_vidc.o(.rev16_text), (4 bytes).
    Removing drv_vidc.o(.revsh_text), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_clear_status0), (14 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_cap_pixel), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_signal_frame), (30 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_int_source), (38 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status0), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status1), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status2), (6 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_dsc_thresh), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_frmst_latency), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_inff_thresh), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_irq_line), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_module_enable), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_outff_thresh), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_update_src_format), (14 bytes).
    Removing irq_redirect .o(.rev16_text), (4 bytes).
    Removing irq_redirect .o(.revsh_text), (4 bytes).
    Removing drv_efuse.o(.rev16_text), (4 bytes).
    Removing drv_efuse.o(.revsh_text), (4 bytes).
    Removing drv_efuse.o(i.drv_efuse_crc_cal), (128 bytes).
    Removing drv_efuse.o(i.drv_efuse_get_default_config), (26 bytes).
    Removing drv_efuse.o(i.drv_efuse_int_disable), (12 bytes).
    Removing drv_efuse.o(i.drv_efuse_write), (46 bytes).
    Removing drv_efuse.o(i.drv_efuse_write_req), (22 bytes).
    Removing drv_phy_common.o(.rev16_text), (4 bytes).
    Removing drv_phy_common.o(.revsh_text), (4 bytes).
    Removing drv_phy_common.o(i.drv_phy_test_read), (8 bytes).
    Removing drv_chip_info.o(.rev16_text), (4 bytes).
    Removing drv_chip_info.o(.revsh_text), (4 bytes).
    Removing drv_dsc_dec.o(.rev16_text), (4 bytes).
    Removing drv_dsc_dec.o(.revsh_text), (4 bytes).
    Removing drv_dsc_dec.o(i.drv_dsc_dec_set_u32_pps), (120 bytes).
    Removing hal_spi_slave.o(.rev16_text), (4 bytes).
    Removing hal_spi_slave.o(.revsh_text), (4 bytes).
    Removing hal_spi_slave.o(i.hal_spi_s_set_high_impedance), (100 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_auto_transfer_abort), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start), (56 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_busy), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_deinit), (10 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_disable), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_enable), (96 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_flush_fifo), (20 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_get_rxfifo_notempty), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_gpio_init), (8 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_init), (76 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_read_data), (10 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_register_callback), (12 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_reset_tx), (68 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_set_auto_rx_buffer), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_set_auto_tx_buffer), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_write_data), (14 bytes).
    Removing norflash.o(.rev16_text), (4 bytes).
    Removing norflash.o(.revsh_text), (4 bytes).
    Removing norflash.o(i.norflash_best_cfg_init), (44 bytes).
    Removing norflash.o(i.norflash_big_end_clear), (14 bytes).
    Removing norflash.o(i.norflash_big_end_enable), (20 bytes).
    Removing norflash.o(i.norflash_check_crc32), (14 bytes).
    Removing norflash.o(i.norflash_check_id), (72 bytes).
    Removing norflash.o(i.norflash_dma_callback), (24 bytes).
    Removing norflash.o(i.norflash_dma_read), (156 bytes).
    Removing norflash.o(i.norflash_dma_write), (252 bytes).
    Removing norflash.o(i.norflash_dual_read), (60 bytes).
    Removing norflash.o(i.norflash_dual_write), (112 bytes).
    Removing norflash.o(i.norflash_en4b), (40 bytes).
    Removing norflash.o(i.norflash_en_quad), (116 bytes).
    Removing norflash.o(i.norflash_en_quad_check), (64 bytes).
    Removing norflash.o(i.norflash_erase_block), (44 bytes).
    Removing norflash.o(i.norflash_erase_chip), (28 bytes).
    Removing norflash.o(i.norflash_erase_sector), (44 bytes).
    Removing norflash.o(i.norflash_ex4b), (40 bytes).
    Removing norflash.o(i.norflash_exit_quad), (76 bytes).
    Removing norflash.o(i.norflash_get_dual_hstatus), (52 bytes).
    Removing norflash.o(i.norflash_get_hstatus), (52 bytes).
    Removing norflash.o(i.norflash_get_status), (52 bytes).
    Removing norflash.o(i.norflash_init), (48 bytes).
    Removing norflash.o(i.norflash_quad_read), (76 bytes).
    Removing norflash.o(i.norflash_quad_write), (108 bytes).
    Removing norflash.o(i.norflash_read), (28 bytes).
    Removing norflash.o(i.norflash_read_config_reg), (36 bytes).
    Removing norflash.o(i.norflash_read_id), (20 bytes).
    Removing norflash.o(i.norflash_read_uid), (52 bytes).
    Removing norflash.o(i.norflash_reset), (2 bytes).
    Removing norflash.o(i.norflash_reset_crc32), (32 bytes).
    Removing norflash.o(i.norflash_set_best_cfg), (50 bytes).
    Removing norflash.o(i.norflash_set_best_read_cfg), (84 bytes).
    Removing norflash.o(i.norflash_set_best_write_cfg), (84 bytes).
    Removing norflash.o(i.norflash_switch_fls_spi), (112 bytes).
    Removing norflash.o(i.norflash_write), (96 bytes).
    Removing norflash.o(i.norflash_write_disable), (64 bytes).
    Removing norflash.o(i.norflash_write_enable), (56 bytes).
    Removing norflash.o(i.norflash_write_endian_scr), (132 bytes).
    Removing norflash.o(.bss), (412 bytes).
    Removing norflash.o(.bss), (32 bytes).
    Removing norflash.o(.data), (2 bytes).
    Removing drv_fls_dma.o(.rev16_text), (4 bytes).
    Removing drv_fls_dma.o(.revsh_text), (4 bytes).
    Removing drv_fls_dma.o(i.fls_abort_dma), (42 bytes).
    Removing drv_fls_dma.o(i.fls_dma_disable), (10 bytes).
    Removing drv_fls_dma.o(i.fls_dma_enable), (10 bytes).
    Removing drv_fls_dma.o(i.fls_dma_read_prepare), (86 bytes).
    Removing drv_fls_dma.o(i.fls_dma_write_prepare), (82 bytes).
    Removing drv_fls_dma.o(i.fls_read_dmacallback), (32 bytes).
    Removing drv_fls_dma.o(i.fls_transfer_create_handle_dma), (208 bytes).
    Removing drv_fls_dma.o(i.fls_transfer_dma), (112 bytes).
    Removing drv_fls_dma.o(i.fls_transfer_get_receive_count_dma), (44 bytes).
    Removing drv_fls_dma.o(i.fls_write_dmacallback), (32 bytes).
    Removing drv_fls_dma.o(.data), (8 bytes).
    Removing drv_pwm.o(.rev16_text), (4 bytes).
    Removing drv_pwm.o(.revsh_text), (4 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_clear_pwm_int_all), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_enable), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_counter_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_current_count), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_high_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_low_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_register_callback), (24 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_set_pwm_int), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_set_sys_int), (64 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_enable), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_get_sync_flag), (16 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_pause), (28 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_control), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_sync_mode), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_threshold), (12 bytes).
    Removing drv_spi_slave.o(.rev16_text), (4 bytes).
    Removing drv_spi_slave.o(.revsh_text), (4 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_deinit), (40 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_disable_int), (68 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_enable_int), (72 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_enable_rx_dma), (32 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_enable_tx_dma), (28 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_get_dma_address), (8 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_gpio_init), (24 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_read_data), (32 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_switch_sclk), (28 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_write_data), (44 bytes).
    Removing drv_spi_slave.o(i.drv_spi_slave_init), (76 bytes).
    Removing drv_swire.o(.rev16_text), (4 bytes).
    Removing drv_swire.o(.revsh_text), (4 bytes).
    Removing drv_swire.o(i.drv_swire_enable), (28 bytes).
    Removing drv_swire.o(i.drv_swire_register_callback), (12 bytes).
    Removing drv_swire.o(i.drv_swire_set_bit_time), (24 bytes).
    Removing drv_swire.o(i.drv_swire_set_power_down), (28 bytes).
    Removing drv_swire.o(i.drv_swire_set_pulse_count), (12 bytes).
    Removing drv_timer.o(.rev16_text), (4 bytes).
    Removing drv_timer.o(.revsh_text), (4 bytes).
    Removing drv_timer.o(i.drv_timer_get_prescaler), (16 bytes).
    Removing drv_timer.o(i.drv_timer_get_status), (38 bytes).
    Removing drv_timer.o(i.drv_timer_register_callback), (20 bytes).
    Removing drv_timer.o(i.drv_timer_set_prescaler), (40 bytes).
    Removing drv_timer.o(i.drv_timer_set_repeat), (16 bytes).
    Removing drv_uart.o(.rev16_text), (4 bytes).
    Removing drv_uart.o(.revsh_text), (4 bytes).
    Removing drv_uart.o(i.UART_AbortReceive), (30 bytes).
    Removing drv_uart.o(i.UART_AbortSend), (30 bytes).
    Removing drv_uart.o(i.UART_Deinit), (28 bytes).
    Removing drv_uart.o(i.UART_Disable_IT), (68 bytes).
    Removing drv_uart.o(i.UART_EnableDma), (32 bytes).
    Removing drv_uart.o(i.UART_Enable_IT), (44 bytes).
    Removing drv_uart.o(i.UART_GetDefaultConfig), (72 bytes).
    Removing drv_uart.o(i.UART_GetFIFO_Ctrl), (20 bytes).
    Removing drv_uart.o(i.UART_GetReceiveCount), (22 bytes).
    Removing drv_uart.o(i.UART_GetReceiveStatus), (20 bytes).
    Removing drv_uart.o(i.UART_GetRxRingBufferLength), (28 bytes).
    Removing drv_uart.o(i.UART_GetSendCount), (22 bytes).
    Removing drv_uart.o(i.UART_GetSendStatus), (20 bytes).
    Removing drv_uart.o(i.UART_ReadBlocking), (32 bytes).
    Removing drv_uart.o(i.UART_ReceiveNonBlocking), (50 bytes).
    Removing drv_uart.o(i.UART_ResetTxFIFO), (36 bytes).
    Removing drv_uart.o(i.UART_SendNonBlocking), (38 bytes).
    Removing drv_uart.o(i.UART_TransferCreateHandle), (96 bytes).
    Removing drv_uart.o(i.UART_TransferStartRingBuffer), (30 bytes).
    Removing drv_uart.o(.constdata), (1 bytes).
    Removing drv_uart_dma.o(.rev16_text), (4 bytes).
    Removing drv_uart_dma.o(.revsh_text), (4 bytes).
    Removing drv_uart_dma.o(i.UART_DMAInit), (76 bytes).
    Removing drv_uart_dma.o(i.UART_TransferAbortReceiveDMA), (16 bytes).
    Removing drv_uart_dma.o(i.UART_TransferAbortSendDMA), (16 bytes).
    Removing drv_uart_dma.o(i.UART_TransferCreateHandleDMA), (176 bytes).
    Removing drv_uart_dma.o(i.UART_TransferGetReceiveCountDMA), (44 bytes).
    Removing drv_uart_dma.o(i.UART_TransferReceiveDMA), (68 bytes).
    Removing drv_uart_dma.o(i.UART_TransferReceiveDMACallback), (34 bytes).
    Removing drv_uart_dma.o(i.UART_TransferSendDMA), (68 bytes).
    Removing drv_uart_dma.o(i.UART_TransferSendDMACallback), (34 bytes).
    Removing drv_uart_dma.o(.data), (8 bytes).
    Removing drv_wdg.o(.rev16_text), (4 bytes).
    Removing drv_wdg.o(.revsh_text), (4 bytes).
    Removing drv_wdg.o(i.drv_wdg_enable), (32 bytes).
    Removing drv_wdg.o(i.drv_wdg_load_match), (12 bytes).
    Removing drv_wdg.o(i.drv_wdg_register_callback), (12 bytes).
    Removing drv_wdg.o(i.drv_wdg_sel_mode), (28 bytes).
    Removing drv_wdg.o(i.drv_wdg_set_repeat), (12 bytes).
    Removing dcs_packet_fifo.o(i.dcs_packet_get_fifo_size), (16 bytes).
    Removing dflti.o(.text), (40 bytes).

713 unused section(s) (total 43127 bytes) removed from the image.

==============================================================================

Image Symbol Table

    Local Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    ../clib/../cmprslib/zerorunl2.c          0x00000000   Number         0  __dczerorl2.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uldiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uidiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  idiv.o ABSOLUTE
    ../clib/microlib/errno.c                 0x00000000   Number         0  errno.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry2.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry5.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8a.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llushr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llshl.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llsshr.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf2.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf6.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf7.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfb.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf0.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf1.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf8.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf3.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf4.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfa.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf5.o ABSOLUTE
    ../clib/microlib/printf/stubs.s          0x00000000   Number         0  stubs.o ABSOLUTE
    ../clib/microlib/stdio/streams.c         0x00000000   Number         0  stdout.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpyb.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpya.o ABSOLUTE
    ../clib/microlib/string/memset.c         0x00000000   Number         0  memseta.o ABSOLUTE
    ../clib/microlib/stubs.s                 0x00000000   Number         0  iusefp.o ABSOLUTE
    ../fplib/microlib/f2d.c                  0x00000000   Number         0  f2d.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  dadd.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  fadd.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  fdiv.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  ddiv.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  fepilogue.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  depilogue.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixui.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixul.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  ffixui.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixi.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  ffixi.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  fflti.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  dfltui.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  ffltui.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  dflti.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  dmul.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  fmul.o ABSOLUTE
    ../fplib/microlib/fpscalb.c              0x00000000   Number         0  fscalb.o ABSOLUTE
    ../fplib/microlib/fpsqrt.c               0x00000000   Number         0  dsqrt.o ABSOLUTE
    ../mathlib/ceil.c                        0x00000000   Number         0  ceil.o ABSOLUTE
    ../mathlib/sqrt.c                        0x00000000   Number         0  sqrt_x.o ABSOLUTE
    ../mathlib/sqrt.c                        0x00000000   Number         0  sqrt.o ABSOLUTE
    ..\..\..\src\common\tau_delay.c          0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\..\..\src\common\tau_log.c            0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\..\..\src\driver\robin\src\drv_chip_info.c 0x00000000   Number         0  drv_chip_info.o ABSOLUTE
    ..\..\..\src\driver\robin\src\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\irq_redirect .c 0x00000000   Number         0  irq_redirect .o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\internal\dcs_packet_fifo.c 0x00000000   Number         0  dcs_packet_fifo.o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\internal\hal_internal_soft_sync.c 0x00000000   Number         0  hal_internal_soft_sync.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_fls.c 0x00000000   Number         0  drv_fls.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_fls_dma.c 0x00000000   Number         0  drv_fls_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_i2c_dma.c 0x00000000   Number         0  drv_i2c_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_i2c_master.c 0x00000000   Number         0  drv_i2c_master.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_i2c_slave.c 0x00000000   Number         0  drv_i2c_slave.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_param_init.c 0x00000000   Number         0  drv_param_init.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_pwm.c 0x00000000   Number         0  drv_pwm.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_spi_dma.c 0x00000000   Number         0  drv_spi_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_spi_master.c 0x00000000   Number         0  drv_spi_master.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_spi_slave.c 0x00000000   Number         0  drv_spi_slave.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_uart_dma.c 0x00000000   Number         0  drv_uart_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_wdg.c 0x00000000   Number         0  drv_wdg.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_i2c_master.c 0x00000000   Number         0  hal_i2c_master.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_i2c_slave.c 0x00000000   Number         0  hal_i2c_slave.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_spi_master.c 0x00000000   Number         0  hal_spi_master.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_spi_slave.c 0x00000000   Number         0  hal_spi_slave.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\internal\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\internal\norflash.c 0x00000000   Number         0  norflash.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_delay.c     0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_log.c       0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\\..\\..\\src\\driver\\robin\\src\\drv_chip_info.c 0x00000000   Number         0  drv_chip_info.o ABSOLUTE
    ..\\..\\..\\src\\driver\\robin\\src\\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\irq_redirect .c 0x00000000   Number         0  irq_redirect .o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\hal\\internal\\hal_internal_soft_sync.c 0x00000000   Number         0  hal_internal_soft_sync.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_fls.c 0x00000000   Number         0  drv_fls.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_fls_dma.c 0x00000000   Number         0  drv_fls_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_i2c_dma.c 0x00000000   Number         0  drv_i2c_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_i2c_master.c 0x00000000   Number         0  drv_i2c_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_i2c_slave.c 0x00000000   Number         0  drv_i2c_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_param_init.c 0x00000000   Number         0  drv_param_init.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_pwm.c 0x00000000   Number         0  drv_pwm.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_spi_dma.c 0x00000000   Number         0  drv_spi_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_spi_master.c 0x00000000   Number         0  drv_spi_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_spi_slave.c 0x00000000   Number         0  drv_spi_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_uart_dma.c 0x00000000   Number         0  drv_uart_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_wdg.c 0x00000000   Number         0  drv_wdg.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_i2c_master.c 0x00000000   Number         0  hal_i2c_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_i2c_slave.c 0x00000000   Number         0  hal_i2c_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_spi_master.c 0x00000000   Number         0  hal_spi_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_spi_slave.c 0x00000000   Number         0  hal_spi_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\internal\\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\internal\\norflash.c 0x00000000   Number         0  norflash.o ABSOLUTE
    ..\\src\\app\\demo\\ap_demo.c            0x00000000   Number         0  ap_demo.o ABSOLUTE
    ..\\src\\app\\demo\\app_tp_for_custom_s8.c 0x00000000   Number         0  app_tp_for_custom_s8.o ABSOLUTE
    ..\\src\\app\\demo\\app_tp_st_touch.c    0x00000000   Number         0  app_tp_st_touch.o ABSOLUTE
    ..\\src\\app\\demo\\app_tp_transfer.c    0x00000000   Number         0  app_tp_transfer.o ABSOLUTE
    ..\\src\\app\\main.c                     0x00000000   Number         0  main.o ABSOLUTE
    ..\\src\\board\\board.c                  0x00000000   Number         0  board.o ABSOLUTE
    ..\src\app\demo\ap_demo.c                0x00000000   Number         0  ap_demo.o ABSOLUTE
    ..\src\app\demo\app_tp_for_custom_s8.c   0x00000000   Number         0  app_tp_for_custom_s8.o ABSOLUTE
    ..\src\app\demo\app_tp_st_touch.c        0x00000000   Number         0  app_tp_st_touch.o ABSOLUTE
    ..\src\app\demo\app_tp_transfer.c        0x00000000   Number         0  app_tp_transfer.o ABSOLUTE
    ..\src\app\main.c                        0x00000000   Number         0  main.o ABSOLUTE
    ..\src\board\board.c                     0x00000000   Number         0  board.o ABSOLUTE
    ..\src\board\startup\startup_ARMCM0.s    0x00000000   Number         0  startup_armcm0.o ABSOLUTE
    cdcmple.s                                0x00000000   Number         0  cdcmple.o ABSOLUTE
    cdrcmple.s                               0x00000000   Number         0  cdrcmple.o ABSOLUTE
    cfcmple.s                                0x00000000   Number         0  cfcmple.o ABSOLUTE
    cfrcmple.s                               0x00000000   Number         0  cfrcmple.o ABSOLUTE
    dc.s                                     0x00000000   Number         0  dc.o ABSOLUTE
    handlers.s                               0x00000000   Number         0  handlers.o ABSOLUTE
    init.s                                   0x00000000   Number         0  init.o ABSOLUTE
    RESET                                    0x00010000   Section      192  startup_armcm0.o(RESET)
    .ARM.Collect$$$$00000000                 0x000100c0   Section        0  entry.o(.ARM.Collect$$$$00000000)
    .ARM.Collect$$$$00000001                 0x000100c0   Section        4  entry2.o(.ARM.Collect$$$$00000001)
    .ARM.Collect$$$$00000004                 0x000100c4   Section        4  entry5.o(.ARM.Collect$$$$00000004)
    .ARM.Collect$$$$00000008                 0x000100c8   Section        0  entry7b.o(.ARM.Collect$$$$00000008)
    .ARM.Collect$$$$0000000A                 0x000100c8   Section        0  entry8b.o(.ARM.Collect$$$$0000000A)
    .ARM.Collect$$$$0000000B                 0x000100c8   Section        8  entry9a.o(.ARM.Collect$$$$0000000B)
    .ARM.Collect$$$$0000000D                 0x000100d0   Section        0  entry10a.o(.ARM.Collect$$$$0000000D)
    .ARM.Collect$$$$0000000F                 0x000100d0   Section        0  entry11a.o(.ARM.Collect$$$$0000000F)
    .ARM.Collect$$$$00002712                 0x000100d0   Section        4  entry2.o(.ARM.Collect$$$$00002712)
    __lit__00000000                          0x000100d0   Data           4  entry2.o(.ARM.Collect$$$$00002712)
    .text                                    0x000100d4   Section      120  startup_armcm0.o(.text)
    .text                                    0x0001014c   Section        0  uidiv.o(.text)
    .text                                    0x00010178   Section        0  idiv.o(.text)
    .text                                    0x000101a0   Section        0  memcpya.o(.text)
    .text                                    0x000101c4   Section        0  memseta.o(.text)
    .text                                    0x000101e8   Section        0  fadd.o(.text)
    .text                                    0x0001029a   Section        0  fmul.o(.text)
    .text                                    0x00010314   Section        0  fdiv.o(.text)
    .text                                    0x00010390   Section        0  fscalb.o(.text)
    .text                                    0x000103a8   Section        0  dadd.o(.text)
    .text                                    0x0001050c   Section        0  dmul.o(.text)
    .text                                    0x000105dc   Section        0  ddiv.o(.text)
    .text                                    0x000106cc   Section        0  fflti.o(.text)
    .text                                    0x000106e2   Section        0  ffltui.o(.text)
    .text                                    0x000106f0   Section        0  dfltui.o(.text)
    .text                                    0x0001070c   Section        0  ffixi.o(.text)
    .text                                    0x0001073e   Section        0  ffixui.o(.text)
    .text                                    0x00010768   Section        0  dfixi.o(.text)
    .text                                    0x000107b0   Section        0  dfixui.o(.text)
    .text                                    0x000107ec   Section        0  f2d.o(.text)
    .text                                    0x00010814   Section       40  cdcmple.o(.text)
    .text                                    0x0001083c   Section       20  cfcmple.o(.text)
    .text                                    0x00010850   Section       20  cfrcmple.o(.text)
    .text                                    0x00010864   Section        0  uldiv.o(.text)
    .text                                    0x000108c4   Section        0  llshl.o(.text)
    .text                                    0x000108e4   Section        0  llushr.o(.text)
    .text                                    0x00010906   Section        0  llsshr.o(.text)
    .text                                    0x0001092c   Section        0  fepilogue.o(.text)
    .text                                    0x0001092c   Section        0  iusefp.o(.text)
    .text                                    0x000109ae   Section        0  depilogue.o(.text)
    .text                                    0x00010a6c   Section        0  dsqrt.o(.text)
    .text                                    0x00010b10   Section        0  dfixul.o(.text)
    .text                                    0x00010b50   Section       40  cdrcmple.o(.text)
    .text                                    0x00010b78   Section       36  init.o(.text)
    .text                                    0x00010b9c   Section        0  __dczerorl2.o(.text)
    i.ADC_IRQn_Handler                       0x00010bf4   Section        0  irq_redirect .o(i.ADC_IRQn_Handler)
    i.AP_NRESET_IRQn_Handler                 0x00010c0c   Section        0  irq_redirect .o(i.AP_NRESET_IRQn_Handler)
    i.DMA_IRQn_Handler                       0x00010c24   Section        0  irq_redirect .o(i.DMA_IRQn_Handler)
    i.EXTI_INT0_IRQn_Handler                 0x00010c38   Section        0  irq_redirect .o(i.EXTI_INT0_IRQn_Handler)
    i.EXTI_INT1_IRQn_Handler                 0x00010c54   Section        0  irq_redirect .o(i.EXTI_INT1_IRQn_Handler)
    i.EXTI_INT2_IRQn_Handler                 0x00010c70   Section        0  irq_redirect .o(i.EXTI_INT2_IRQn_Handler)
    i.EXTI_INT3_IRQn_Handler                 0x00010c8c   Section        0  irq_redirect .o(i.EXTI_INT3_IRQn_Handler)
    i.EXTI_INT4_IRQn_Handler                 0x00010ca8   Section        0  irq_redirect .o(i.EXTI_INT4_IRQn_Handler)
    i.EXTI_INT5_IRQn_Handler                 0x00010cc4   Section        0  irq_redirect .o(i.EXTI_INT5_IRQn_Handler)
    i.EXTI_INT6_IRQn_Handler                 0x00010ce0   Section        0  irq_redirect .o(i.EXTI_INT6_IRQn_Handler)
    i.EXTI_INT7_IRQn_Handler                 0x00010cfc   Section        0  irq_redirect .o(i.EXTI_INT7_IRQn_Handler)
    i.FLSCTRL_IRQn_Handler                   0x00010d18   Section        0  irq_redirect .o(i.FLSCTRL_IRQn_Handler)
    i.Gpio_swire_output                      0x00010d2c   Section        0  ap_demo.o(i.Gpio_swire_output)
    i.HardFault_Handler                      0x00010d7c   Section        0  irq_redirect .o(i.HardFault_Handler)
    i.I2C0_IRQn_Handler                      0x00010d90   Section        0  irq_redirect .o(i.I2C0_IRQn_Handler)
    i.I2C1_IRQn_Handler                      0x00010da8   Section        0  irq_redirect .o(i.I2C1_IRQn_Handler)
    i.LCDC_IRQn_Handler                      0x00010dc0   Section        0  irq_redirect .o(i.LCDC_IRQn_Handler)
    i.LOG_printf                             0x00010dd8   Section        0  tau_log.o(i.LOG_printf)
    i.MEMC_IRQn_Handler                      0x00010e00   Section        0  irq_redirect .o(i.MEMC_IRQn_Handler)
    i.MIPI_RX_IRQn_Handler                   0x00010e18   Section        0  irq_redirect .o(i.MIPI_RX_IRQn_Handler)
    i.MIPI_TX_IRQn_Handler                   0x00010e30   Section        0  irq_redirect .o(i.MIPI_TX_IRQn_Handler)
    i.PWMDET_IRQn_Handler                    0x00010e48   Section        0  irq_redirect .o(i.PWMDET_IRQn_Handler)
    i.SPIM_IRQn_Handler                      0x00010e64   Section        0  irq_redirect .o(i.SPIM_IRQn_Handler)
    i.SPIS_IRQn_Handler                      0x00010e80   Section        0  irq_redirect .o(i.SPIS_IRQn_Handler)
    i.SWIRE_IRQn_Handler                     0x00010e9c   Section        0  irq_redirect .o(i.SWIRE_IRQn_Handler)
    i.SysTick_Handler                        0x00010eb8   Section        0  irq_redirect .o(i.SysTick_Handler)
    i.TIMER0_IRQn_Handler                    0x00010ed0   Section        0  irq_redirect .o(i.TIMER0_IRQn_Handler)
    i.TIMER1_IRQn_Handler                    0x00010ee8   Section        0  irq_redirect .o(i.TIMER1_IRQn_Handler)
    i.TIMER2_IRQn_Handler                    0x00010f00   Section        0  irq_redirect .o(i.TIMER2_IRQn_Handler)
    i.TIMER3_IRQn_Handler                    0x00010f18   Section        0  irq_redirect .o(i.TIMER3_IRQn_Handler)
    i.UART0_IRQ_Handle                       0x00010f30   Section        0  drv_uart.o(i.UART0_IRQ_Handle)
    i.UART_DisableDma                        0x00010f4c   Section        0  drv_uart.o(i.UART_DisableDma)
    i.UART_GetInstance                       0x00010f4e   Section        0  drv_uart.o(i.UART_GetInstance)
    i.UART_IRQn_Handler                      0x00010f54   Section        0  irq_redirect .o(i.UART_IRQn_Handler)
    i.UART_ResetRxFIFO                       0x00010f6c   Section        0  drv_uart.o(i.UART_ResetRxFIFO)
    i.UART_SetBaudRate                       0x00010f90   Section        0  drv_uart.o(i.UART_SetBaudRate)
    i.UART_SwitchSCLK                        0x00010fd8   Section        0  drv_uart.o(i.UART_SwitchSCLK)
    i.__scatterload_copy                     0x00010ff2   Section       14  handlers.o(i.__scatterload_copy)
    .ARM.__at_0x11000                        0x00011000   Section       20  drv_common.o(.ARM.__at_0x11000)
    i.__scatterload_null                     0x00011014   Section        2  handlers.o(i.__scatterload_null)
    .ARM.__at_0x11018                        0x00011018   Section        4  drv_common.o(.ARM.__at_0x11018)
    i.UART_TransferHandleIRQ                 0x0001101c   Section        0  drv_uart.o(i.UART_TransferHandleIRQ)
    i.UART_WriteBlocking                     0x00011150   Section        0  drv_uart.o(i.UART_WriteBlocking)
    i.UART_init                              0x0001116c   Section        0  drv_uart.o(i.UART_init)
    i.VIDC_IRQn_Handler                      0x00011228   Section        0  irq_redirect .o(i.VIDC_IRQn_Handler)
    i.VPRE_IRQn_Handler                      0x00011240   Section        0  irq_redirect .o(i.VPRE_IRQn_Handler)
    i.WDG_IRQn_Handler                       0x00011258   Section        0  irq_redirect .o(i.WDG_IRQn_Handler)
    i.__0printf                              0x00011270   Section        0  printfa.o(i.__0printf)
    i.__0vsprintf                            0x00011290   Section        0  printfa.o(i.__0vsprintf)
    i.__ARM_clz                              0x000112b4   Section        0  depilogue.o(i.__ARM_clz)
    i.__ARM_common_switch8                   0x000112e2   Section        0  hal_dsi_rx_ctrl.o(i.__ARM_common_switch8)
    i.__NVIC_ClearPendingIRQ                 0x000112fc   Section        0  drv_spi_master.o(i.__NVIC_ClearPendingIRQ)
    __NVIC_ClearPendingIRQ                   0x000112fd   Thumb Code    18  drv_spi_master.o(i.__NVIC_ClearPendingIRQ)
    i.__NVIC_DisableIRQ                      0x00011314   Section        0  drv_rxbr.o(i.__NVIC_DisableIRQ)
    __NVIC_DisableIRQ                        0x00011315   Thumb Code    26  drv_rxbr.o(i.__NVIC_DisableIRQ)
    i.__NVIC_EnableIRQ                       0x00011334   Section        0  drv_rxbr.o(i.__NVIC_EnableIRQ)
    __NVIC_EnableIRQ                         0x00011335   Thumb Code    18  drv_rxbr.o(i.__NVIC_EnableIRQ)
    i.__NVIC_SetPriority                     0x0001134c   Section        0  hal_spi_slave.o(i.__NVIC_SetPriority)
    __NVIC_SetPriority                       0x0001134d   Thumb Code    60  hal_spi_slave.o(i.__NVIC_SetPriority)
    i.__scatterload_zeroinit                 0x00011390   Section       14  handlers.o(i.__scatterload_zeroinit)
    i.__set_errno                            0x000113a0   Section        0  errno.o(i.__set_errno)
    i._fp_digits                             0x000113ac   Section        0  printfa.o(i._fp_digits)
    _fp_digits                               0x000113ad   Thumb Code   344  printfa.o(i._fp_digits)
    i._printf_core                           0x00011520   Section        0  printfa.o(i._printf_core)
    _printf_core                             0x00011521   Thumb Code  1754  printfa.o(i._printf_core)
    i._printf_post_padding                   0x00011c0c   Section        0  printfa.o(i._printf_post_padding)
    _printf_post_padding                     0x00011c0d   Thumb Code    32  printfa.o(i._printf_post_padding)
    i._printf_pre_padding                    0x00011c2c   Section        0  printfa.o(i._printf_pre_padding)
    _printf_pre_padding                      0x00011c2d   Thumb Code    44  printfa.o(i._printf_pre_padding)
    i._sputc                                 0x00011c58   Section        0  printfa.o(i._sputc)
    _sputc                                   0x00011c59   Thumb Code    10  printfa.o(i._sputc)
    i.ap_dcs_read                            0x00011c64   Section        0  ap_demo.o(i.ap_dcs_read)
    ap_dcs_read                              0x00011c65   Thumb Code  4158  ap_demo.o(i.ap_dcs_read)
    i.ap_demo                                0x00012cdc   Section        0  ap_demo.o(i.ap_demo)
    i.ap_get_reg_df                          0x00012dfc   Section        0  ap_demo.o(i.ap_get_reg_df)
    ap_get_reg_df                            0x00012dfd   Thumb Code    68  ap_demo.o(i.ap_get_reg_df)
    i.ap_get_tp_calibration_status_01        0x00012e48   Section        0  app_tp_st_touch.o(i.ap_get_tp_calibration_status_01)
    i.ap_set_backlight_51                    0x00012e68   Section        0  ap_demo.o(i.ap_set_backlight_51)
    ap_set_backlight_51                      0x00012e69   Thumb Code    76  ap_demo.o(i.ap_set_backlight_51)
    i.ap_set_display_off                     0x00012edc   Section        0  ap_demo.o(i.ap_set_display_off)
    ap_set_display_off                       0x00012edd   Thumb Code    28  ap_demo.o(i.ap_set_display_off)
    i.ap_set_display_on                      0x00012f20   Section        0  ap_demo.o(i.ap_set_display_on)
    ap_set_display_on                        0x00012f21   Thumb Code    16  ap_demo.o(i.ap_set_display_on)
    i.ap_set_enter_sleep_mode                0x00012f58   Section        0  ap_demo.o(i.ap_set_enter_sleep_mode)
    ap_set_enter_sleep_mode                  0x00012f59   Thumb Code    74  ap_demo.o(i.ap_set_enter_sleep_mode)
    i.ap_set_exit_sleep_mode                 0x00012fd8   Section        0  ap_demo.o(i.ap_set_exit_sleep_mode)
    ap_set_exit_sleep_mode                   0x00012fd9   Thumb Code    58  ap_demo.o(i.ap_set_exit_sleep_mode)
    i.ap_set_hbm_53                          0x00013048   Section        0  ap_demo.o(i.ap_set_hbm_53)
    ap_set_hbm_53                            0x00013049   Thumb Code    44  ap_demo.o(i.ap_set_hbm_53)
    i.ap_update_frame_rate                   0x00013078   Section        0  ap_demo.o(i.ap_update_frame_rate)
    ap_update_frame_rate                     0x00013079   Thumb Code    36  ap_demo.o(i.ap_update_frame_rate)
    i.app_ADC_IRQn_Handler                   0x000130a0   Section        0  drv_rxbr.o(i.app_ADC_IRQn_Handler)
    i.app_AP_NRESET_IRQn_Handler             0x000130bc   Section        0  drv_gpio.o(i.app_AP_NRESET_IRQn_Handler)
    i.app_EXTI_INT0_IRQn_Handler             0x000130e0   Section        0  drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler)
    i.app_EXTI_INT1_IRQn_Handler             0x000130fc   Section        0  drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler)
    i.app_EXTI_INT2_IRQn_Handler             0x00013118   Section        0  drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler)
    i.app_EXTI_INT3_IRQn_Handler             0x00013134   Section        0  drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler)
    i.app_EXTI_INT4_IRQn_Handler             0x00013150   Section        0  drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler)
    i.app_EXTI_INT5_IRQn_Handler             0x0001316c   Section        0  drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler)
    i.app_EXTI_INT6_IRQn_Handler             0x00013188   Section        0  drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler)
    i.app_EXTI_INT7_IRQn_Handler             0x000131a4   Section        0  drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler)
    i.app_HardFault_Handler                  0x000131c0   Section        0  drv_common.o(i.app_HardFault_Handler)
    i.app_I2C0_IRQn_Handler                  0x00013208   Section        0  drv_i2c_slave.o(i.app_I2C0_IRQn_Handler)
    i.app_I2C1_IRQn_Handler                  0x00013220   Section        0  drv_i2c_master.o(i.app_I2C1_IRQn_Handler)
    i.app_LCDC_IRQn_Handler                  0x00013230   Section        0  hal_internal_vsync.o(i.app_LCDC_IRQn_Handler)
    i.app_MEMC_IRQn_Handler                  0x00013360   Section        0  drv_memc.o(i.app_MEMC_IRQn_Handler)
    i.app_MIPI_RX_IRQn_Handler               0x000133e8   Section        0  drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler)
    i.app_MIPI_TX_IRQn_Handler               0x00013680   Section        0  drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler)
    i.app_PWMDET_IRQn_Handler                0x00013720   Section        0  drv_pwm.o(i.app_PWMDET_IRQn_Handler)
    i.app_SPIM_IRQn_Handler                  0x00013768   Section        0  drv_spi_master.o(i.app_SPIM_IRQn_Handler)
    i.app_SPIS_IRQn_Handler                  0x00013798   Section        0  hal_spi_slave.o(i.app_SPIS_IRQn_Handler)
    i.app_SWIRE_IRQn_Handler                 0x00013998   Section        0  drv_swire.o(i.app_SWIRE_IRQn_Handler)
    i.app_SysTick_Handler                    0x000139b8   Section        0  drv_common.o(i.app_SysTick_Handler)
    i.app_TIMER0_IRQn_Handler                0x000139d0   Section        0  drv_timer.o(i.app_TIMER0_IRQn_Handler)
    i.app_TIMER1_IRQn_Handler                0x000139da   Section        0  drv_timer.o(i.app_TIMER1_IRQn_Handler)
    i.app_TIMER2_IRQn_Handler                0x000139e4   Section        0  drv_timer.o(i.app_TIMER2_IRQn_Handler)
    i.app_TIMER3_IRQn_Handler                0x000139ee   Section        0  drv_timer.o(i.app_TIMER3_IRQn_Handler)
    i.app_UART_IRQn_Handler                  0x000139f8   Section        0  drv_uart.o(i.app_UART_IRQn_Handler)
    i.app_VIDC_IRQn_Handler                  0x00013a00   Section        0  drv_vidc.o(i.app_VIDC_IRQn_Handler)
    i.app_VPRE_IRQn_Handler                  0x00013a1c   Section        0  drv_rxbr.o(i.app_VPRE_IRQn_Handler)
    i.app_WDG_IRQn_Handler                   0x00013a38   Section        0  drv_wdg.o(i.app_WDG_IRQn_Handler)
    i.app_dma_irq_handler                    0x00013a70   Section        0  drv_dma.o(i.app_dma_irq_handler)
    i.app_fls_ctrl_Handler                   0x00013a80   Section        0  norflash.o(i.app_fls_ctrl_Handler)
    i.board_Init                             0x00013ab0   Section        0  board.o(i.board_Init)
    i.calc_framebuffer_setting               0x00013ad4   Section        0  hal_internal_vsync.o(i.calc_framebuffer_setting)
    i.ceil                                   0x00014060   Section        0  ceil.o(i.ceil)
    i.check_mipi_rx_tx_video_info            0x00014128   Section        0  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    check_mipi_rx_tx_video_info              0x00014129   Thumb Code    44  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    i.check_pkt_buf_rev                      0x00014154   Section        0  hal_internal_vsync.o(i.check_pkt_buf_rev)
    check_pkt_buf_rev                        0x00014155   Thumb Code    74  hal_internal_vsync.o(i.check_pkt_buf_rev)
    i.dcs_packet_fifo_alloc                  0x000141d8   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    i.dcs_packet_fifo_init                   0x00014230   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    i.dcs_packet_free_fifo_header            0x00014248   Section        0  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    i.dcs_packet_get_fifo_header             0x0001428c   Section        0  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    i.dcs_sw_filter                          0x000142b0   Section        0  hal_internal_vsync.o(i.dcs_sw_filter)
    dcs_sw_filter                            0x000142b1   Thumb Code    36  hal_internal_vsync.o(i.dcs_sw_filter)
    i.delayMs                                0x000142dc   Section        0  tau_delay.o(i.delayMs)
    i.delayUs                                0x000142f4   Section        0  tau_delay.o(i.delayUs)
    i.drv_ap_rst_trig_edge_detect            0x00014318   Section        0  drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect)
    i.drv_chip_info_get_info                 0x00014350   Section        0  drv_chip_info.o(i.drv_chip_info_get_info)
    i.drv_chip_info_init                     0x0001435c   Section        0  drv_chip_info.o(i.drv_chip_info_init)
    i.drv_chip_rx_info_check                 0x0001439c   Section        0  drv_chip_info.o(i.drv_chip_rx_info_check)
    i.drv_chip_rx_init_done                  0x0001444c   Section        0  drv_chip_info.o(i.drv_chip_rx_init_done)
    i.drv_common_enable_systick              0x00014460   Section        0  drv_common.o(i.drv_common_enable_systick)
    i.drv_common_system_init                 0x000144b8   Section        0  drv_common.o(i.drv_common_system_init)
    i.drv_crgu_config_reset_modules          0x000144c0   Section        0  drv_crgu.o(i.drv_crgu_config_reset_modules)
    i.drv_crgu_set_ahb_pre_div               0x000144d0   Section        0  drv_crgu.o(i.drv_crgu_set_ahb_pre_div)
    i.drv_crgu_set_ahb_src                   0x000144e4   Section        0  drv_crgu.o(i.drv_crgu_set_ahb_src)
    i.drv_crgu_set_clock                     0x000144f8   Section        0  drv_crgu.o(i.drv_crgu_set_clock)
    i.drv_crgu_set_dpi_mux_src               0x00014518   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_mux_src)
    i.drv_crgu_set_dpi_pre_div               0x0001452c   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_pre_div)
    i.drv_crgu_set_dpi_pre_src               0x00014544   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_pre_src)
    i.drv_crgu_set_dsc_core_div              0x00014558   Section        0  drv_crgu.o(i.drv_crgu_set_dsc_core_div)
    i.drv_crgu_set_dsco_src                  0x0001456c   Section        0  drv_crgu.o(i.drv_crgu_set_dsco_src)
    i.drv_crgu_set_dsco_src_div              0x00014580   Section        0  drv_crgu.o(i.drv_crgu_set_dsco_src_div)
    i.drv_crgu_set_fb_div                    0x00014594   Section        0  drv_crgu.o(i.drv_crgu_set_fb_div)
    i.drv_crgu_set_fb_src                    0x000145a8   Section        0  drv_crgu.o(i.drv_crgu_set_fb_src)
    i.drv_crgu_set_lcdc_div                  0x000145bc   Section        0  drv_crgu.o(i.drv_crgu_set_lcdc_div)
    i.drv_crgu_set_lcdc_src                  0x000145d0   Section        0  drv_crgu.o(i.drv_crgu_set_lcdc_src)
    i.drv_crgu_set_mipi_cfg_src              0x000145e4   Section        0  drv_crgu.o(i.drv_crgu_set_mipi_cfg_src)
    i.drv_crgu_set_mipi_ref_src              0x000145f8   Section        0  drv_crgu.o(i.drv_crgu_set_mipi_ref_src)
    i.drv_crgu_set_reset                     0x00014610   Section        0  drv_crgu.o(i.drv_crgu_set_reset)
    i.drv_crgu_set_rxbr_div                  0x00014628   Section        0  drv_crgu.o(i.drv_crgu_set_rxbr_div)
    i.drv_crgu_set_rxbr_src                  0x0001463c   Section        0  drv_crgu.o(i.drv_crgu_set_rxbr_src)
    i.drv_crgu_set_vidc_src                  0x00014650   Section        0  drv_crgu.o(i.drv_crgu_set_vidc_src)
    i.drv_dma_clear_flag                     0x00014664   Section        0  drv_dma.o(i.drv_dma_clear_flag)
    i.drv_dma_get_channel_flag               0x0001467c   Section        0  drv_dma.o(i.drv_dma_get_channel_flag)
    i.drv_dma_irq_handler                    0x00014688   Section        0  drv_dma.o(i.drv_dma_irq_handler)
    i.drv_dsc_dec_convert_pps_rc_parameter   0x00014718   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter)
    i.drv_dsc_dec_disable                    0x0001474e   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    i.drv_dsc_dec_enable                     0x0001475c   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    i.drv_dsc_dec_get_nslc                   0x000147d0   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    i.drv_dsc_dec_set_u8_pps                 0x000147da   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps)
    i.drv_dsi_rx_calc_ipi_tx_delay           0x00014804   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    i.drv_dsi_rx_enable_irq                  0x00014908   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    i.drv_dsi_rx_get_bta_status              0x00014948   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_bta_status)
    i.drv_dsi_rx_get_color_bpp               0x00014958   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    drv_dsi_rx_get_color_bpp                 0x00014959   Thumb Code    62  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    i.drv_dsi_rx_get_color_pcc               0x000149a8   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    drv_dsi_rx_get_color_pcc                 0x000149a9   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    i.drv_dsi_rx_get_compression_en          0x000149c4   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    i.drv_dsi_rx_get_max_ret_size            0x000149cc   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size)
    i.drv_dsi_rx_power_up                    0x000149d2   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    i.drv_dsi_rx_set_ctrl_cfg                0x000149e0   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    i.drv_dsi_rx_set_ddi_cfg                 0x00014a00   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    i.drv_dsi_rx_set_inten                   0x00014a10   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    i.drv_dsi_rx_set_ipi_cfg                 0x00014a14   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    i.drv_dsi_rx_set_lane_swap               0x00014a24   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    i.drv_dsi_rx_set_resp_cnt                0x00014a6a   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    i.drv_dsi_rx_set_up_phy                  0x00014a90   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    i.drv_dsi_rx_shut_down                   0x00014b94   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    i.drv_dsi_tx_command_header              0x00014ba2   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    i.drv_dsi_tx_command_mode_cfg            0x00014bb6   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    i.drv_dsi_tx_command_put_payload         0x00014c22   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    i.drv_dsi_tx_config_eotp                 0x00014c26   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    i.drv_dsi_tx_config_int                  0x00014c3e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    i.drv_dsi_tx_dpi_lpcmd_time              0x00014c46   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    i.drv_dsi_tx_dpi_mode                    0x00014c4e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    i.drv_dsi_tx_dpi_polarity                0x00014c58   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    i.drv_dsi_tx_edpi_cmd_size               0x00014c7c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    i.drv_dsi_tx_get_cmd_status              0x00014c80   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    i.drv_dsi_tx_mode                        0x00014c84   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    i.drv_dsi_tx_phy_clock_lane_auto_lp      0x00014c88   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    i.drv_dsi_tx_phy_clock_lane_req_hs       0x00014ca0   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    i.drv_dsi_tx_phy_lane_mode               0x00014cba   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    i.drv_dsi_tx_phy_status_ready            0x00014cc6   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    i.drv_dsi_tx_phy_status_stopstate        0x00014d2a   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    i.drv_dsi_tx_phy_test_setup              0x00014d68   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    i.drv_dsi_tx_phy_time_cfg                0x00014e9c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    i.drv_dsi_tx_powerup                     0x00014eba   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    i.drv_dsi_tx_response_mode               0x00014ec2   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    i.drv_dsi_tx_set_bta_ack                 0x00014ede   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    i.drv_dsi_tx_set_esc_div                 0x00014ef6   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    i.drv_dsi_tx_set_int                     0x00014f04   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    i.drv_dsi_tx_set_time_out_div            0x00014f44   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    i.drv_dsi_tx_set_video_chunk             0x00014f54   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    i.drv_dsi_tx_set_video_timing            0x00014f5c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    i.drv_dsi_tx_shutdown                    0x00014f7e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    i.drv_dsi_tx_timeout_cfg                 0x00014f86   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    i.drv_dsi_tx_video_mode_cfg              0x00014fac   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    i.drv_dsi_tx_video_mode_disable_hact_cmd 0x00015056   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_disable_hact_cmd)
    i.drv_dsi_tx_video_mode_set_lp_cmd       0x0001506c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd)
    i.drv_efuse_enter_inactive               0x00015084   Section        0  drv_efuse.o(i.drv_efuse_enter_inactive)
    i.drv_efuse_int_enable                   0x000150b2   Section        0  drv_efuse.o(i.drv_efuse_int_enable)
    i.drv_efuse_read                         0x000150be   Section        0  drv_efuse.o(i.drv_efuse_read)
    i.drv_efuse_read_req                     0x000150f0   Section        0  drv_efuse.o(i.drv_efuse_read_req)
    i.drv_gpio_set_ioe                       0x00015108   Section        0  drv_gpio.o(i.drv_gpio_set_ioe)
    i.drv_gpio_set_mode0                     0x00015128   Section        0  drv_gpio.o(i.drv_gpio_set_mode0)
    i.drv_gpio_set_mode1                     0x00015138   Section        0  drv_gpio.o(i.drv_gpio_set_mode1)
    i.drv_gpio_set_mode2                     0x00015148   Section        0  drv_gpio.o(i.drv_gpio_set_mode2)
    i.drv_gpio_set_mode3                     0x00015158   Section        0  drv_gpio.o(i.drv_gpio_set_mode3)
    i.drv_gpio_set_output_data               0x00015168   Section        0  hal_gpio.o(i.drv_gpio_set_output_data)
    drv_gpio_set_output_data                 0x00015169   Thumb Code    26  hal_gpio.o(i.drv_gpio_set_output_data)
    i.drv_lcdc_config_bypass                 0x00015188   Section        0  drv_lcdc.o(i.drv_lcdc_config_bypass)
    i.drv_lcdc_config_ccm                    0x000151a0   Section        0  drv_lcdc.o(i.drv_lcdc_config_ccm)
    i.drv_lcdc_config_disp_mode              0x000151d0   Section        0  drv_lcdc.o(i.drv_lcdc_config_disp_mode)
    i.drv_lcdc_config_dpi_polarity           0x000151e6   Section        0  drv_lcdc.o(i.drv_lcdc_config_dpi_polarity)
    i.drv_lcdc_config_dpi_timing             0x0001520a   Section        0  drv_lcdc.o(i.drv_lcdc_config_dpi_timing)
    i.drv_lcdc_config_edpi_mode              0x00015230   Section        0  drv_lcdc.o(i.drv_lcdc_config_edpi_mode)
    i.drv_lcdc_config_endianness             0x00015246   Section        0  drv_lcdc.o(i.drv_lcdc_config_endianness)
    i.drv_lcdc_config_input_size             0x0001525c   Section        0  drv_lcdc.o(i.drv_lcdc_config_input_size)
    i.drv_lcdc_config_int                    0x00015268   Section        0  drv_lcdc.o(i.drv_lcdc_config_int)
    i.drv_lcdc_config_int_single             0x00015286   Section        0  drv_lcdc.o(i.drv_lcdc_config_int_single)
    i.drv_lcdc_config_overwrite              0x000152a8   Section        0  drv_lcdc.o(i.drv_lcdc_config_overwrite)
    i.drv_lcdc_config_overwrite_rgb          0x000152ca   Section        0  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    i.drv_lcdc_config_partial_display_area   0x000152d6   Section        0  drv_lcdc.o(i.drv_lcdc_config_partial_display_area)
    i.drv_lcdc_config_partial_display_enable 0x000152f0   Section        0  drv_lcdc.o(i.drv_lcdc_config_partial_display_enable)
    i.drv_lcdc_config_scale_up_coef          0x00015312   Section        0  drv_lcdc.o(i.drv_lcdc_config_scale_up_coef)
    i.drv_lcdc_config_scale_up_step          0x0001532c   Section        0  drv_lcdc.o(i.drv_lcdc_config_scale_up_step)
    i.drv_lcdc_config_src_parameter          0x00015338   Section        0  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    i.drv_lcdc_config_thresh                 0x00015384   Section        0  drv_lcdc.o(i.drv_lcdc_config_thresh)
    i.drv_lcdc_ctrl_flow                     0x0001538a   Section        0  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    i.drv_lcdc_enable_shadow_reg             0x0001539c   Section        0  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    i.drv_lcdc_set_int                       0x000153bc   Section        0  drv_lcdc.o(i.drv_lcdc_set_int)
    i.drv_lcdc_set_prefetch                  0x000153fc   Section        0  drv_lcdc.o(i.drv_lcdc_set_prefetch)
    i.drv_lcdc_set_video_hw_mode             0x00015414   Section        0  drv_lcdc.o(i.drv_lcdc_set_video_hw_mode)
    i.drv_lcdc_start                         0x00015428   Section        0  drv_lcdc.o(i.drv_lcdc_start)
    i.drv_memc_clear_status                  0x00015448   Section        0  drv_memc.o(i.drv_memc_clear_status)
    i.drv_memc_enable_irq                    0x00015454   Section        0  drv_memc.o(i.drv_memc_enable_irq)
    i.drv_memc_gen_a_tear_signal             0x00015494   Section        0  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    i.drv_memc_get_status                    0x000154a0   Section        0  drv_memc.o(i.drv_memc_get_status)
    i.drv_memc_rate_transfer_sel             0x000154b2   Section        0  drv_memc.o(i.drv_memc_rate_transfer_sel)
    i.drv_memc_sel_vsync                     0x000154c2   Section        0  drv_memc.o(i.drv_memc_sel_vsync)
    i.drv_memc_set_active_height             0x000154d0   Section        0  drv_memc.o(i.drv_memc_set_active_height)
    i.drv_memc_set_data_mode                 0x000154e4   Section        0  drv_memc.o(i.drv_memc_set_data_mode)
    i.drv_memc_set_double_buffer             0x000154f0   Section        0  drv_memc.o(i.drv_memc_set_double_buffer)
    i.drv_memc_set_double_buffer_reverse     0x00015500   Section        0  drv_memc.o(i.drv_memc_set_double_buffer_reverse)
    i.drv_memc_set_fs_en_conditions          0x00015512   Section        0  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    i.drv_memc_set_inten                     0x00015522   Section        0  drv_memc.o(i.drv_memc_set_inten)
    i.drv_memc_set_lcdc_st_conditions        0x00015538   Section        0  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    i.drv_memc_set_ltpo_mode                 0x00015550   Section        0  drv_memc.o(i.drv_memc_set_ltpo_mode)
    i.drv_memc_set_tear_mode                 0x0001556a   Section        0  drv_memc.o(i.drv_memc_set_tear_mode)
    i.drv_memc_set_tear_waveform             0x00015578   Section        0  drv_memc.o(i.drv_memc_set_tear_waveform)
    i.drv_memc_set_vidc_sync_cnt             0x000155a0   Section        0  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    i.drv_param_init_get_ccm                 0x000155b0   Section        0  drv_param_init.o(i.drv_param_init_get_ccm)
    i.drv_param_init_get_scld_filter_h       0x000155b8   Section        0  drv_param_init.o(i.drv_param_init_get_scld_filter_h)
    i.drv_param_init_get_scld_filter_v       0x000155cc   Section        0  drv_param_init.o(i.drv_param_init_get_scld_filter_v)
    i.drv_param_init_get_sclu_filter         0x000155e0   Section        0  drv_param_init.o(i.drv_param_init_get_sclu_filter)
    i.drv_param_init_set_ccm                 0x000155e8   Section        0  drv_param_init.o(i.drv_param_init_set_ccm)
    i.drv_param_init_set_scld_filter         0x000155fc   Section        0  drv_param_init.o(i.drv_param_init_set_scld_filter)
    i.drv_param_p2r_filter_init              0x00015660   Section        0  drv_param_init.o(i.drv_param_p2r_filter_init)
    i.drv_phy_enable_calibration             0x00015684   Section        0  drv_phy_common.o(i.drv_phy_enable_calibration)
    i.drv_phy_get_calibration                0x00015694   Section        0  drv_phy_common.o(i.drv_phy_get_calibration)
    i.drv_phy_get_pll_para                   0x000156d0   Section        0  drv_phy_common.o(i.drv_phy_get_pll_para)
    i.drv_phy_get_rate_para                  0x00015730   Section        0  drv_phy_common.o(i.drv_phy_get_rate_para)
    i.drv_phy_test_clear                     0x00015784   Section        0  drv_phy_common.o(i.drv_phy_test_clear)
    i.drv_phy_test_lock                      0x00015794   Section        0  drv_phy_common.o(i.drv_phy_test_lock)
    i.drv_phy_test_write_1_byte              0x000157ac   Section        0  drv_phy_common.o(i.drv_phy_test_write_1_byte)
    i.drv_phy_test_write_2_byte              0x000157cc   Section        0  drv_phy_common.o(i.drv_phy_test_write_2_byte)
    i.drv_phy_test_write_code                0x000157f2   Section        0  drv_phy_common.o(i.drv_phy_test_write_code)
    i.drv_phy_test_write_data                0x00015810   Section        0  drv_phy_common.o(i.drv_phy_test_write_data)
    drv_phy_test_write_data                  0x00015811   Thumb Code    32  drv_phy_common.o(i.drv_phy_test_write_data)
    i.drv_pwr_set_pvd_mode                   0x00015830   Section        0  drv_pwr.o(i.drv_pwr_set_pvd_mode)
    i.drv_pwr_set_system_clk_src             0x00015848   Section        0  drv_pwr.o(i.drv_pwr_set_system_clk_src)
    i.drv_rx_phy_test_clear                  0x00015880   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_clear)
    drv_rx_phy_test_clear                    0x00015881   Thumb Code    12  drv_dsi_rx.o(i.drv_rx_phy_test_clear)
    i.drv_rx_phy_test_lock                   0x0001588c   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_lock)
    drv_rx_phy_test_lock                     0x0001588d   Thumb Code    16  drv_dsi_rx.o(i.drv_rx_phy_test_lock)
    i.drv_rx_phy_test_write_1_byte           0x0001589c   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte)
    drv_rx_phy_test_write_1_byte             0x0001589d   Thumb Code    20  drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte)
    i.drv_rx_phy_test_write_2_byte           0x000158b0   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte)
    drv_rx_phy_test_write_2_byte             0x000158b1   Thumb Code    22  drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte)
    i.drv_rxbr_clear_pkt_buffer              0x000158c6   Section        0  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    i.drv_rxbr_clear_status0                 0x000158d0   Section        0  drv_rxbr.o(i.drv_rxbr_clear_status0)
    i.drv_rxbr_enable_irq                    0x000158d4   Section        0  drv_rxbr.o(i.drv_rxbr_enable_irq)
    i.drv_rxbr_frame_drop_cfg                0x00015930   Section        0  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    i.drv_rxbr_get_clk                       0x00015944   Section        0  drv_rxbr.o(i.drv_rxbr_get_clk)
    i.drv_rxbr_get_col_addr                  0x000159a8   Section        0  drv_rxbr.o(i.drv_rxbr_get_col_addr)
    i.drv_rxbr_get_int_source                0x000159ac   Section        0  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    drv_rxbr_get_int_source                  0x000159ad   Thumb Code    18  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    i.drv_rxbr_get_page_addr                 0x000159be   Section        0  drv_rxbr.o(i.drv_rxbr_get_page_addr)
    i.drv_rxbr_get_pkt_buf_error_status      0x000159c2   Section        0  drv_rxbr.o(i.drv_rxbr_get_pkt_buf_error_status)
    i.drv_rxbr_get_status0                   0x000159ce   Section        0  hal_internal_vsync.o(i.drv_rxbr_get_status0)
    drv_rxbr_get_status0                     0x000159cf   Thumb Code    18  hal_internal_vsync.o(i.drv_rxbr_get_status0)
    i.drv_rxbr_get_status1                   0x000159e0   Section        0  hal_internal_vsync.o(i.drv_rxbr_get_status1)
    drv_rxbr_get_status1                     0x000159e1   Thumb Code    22  hal_internal_vsync.o(i.drv_rxbr_get_status1)
    i.drv_rxbr_hline_rcv0_cfg                0x000159f6   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg)
    i.drv_rxbr_hline_rcv1_cfg                0x00015a02   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg)
    i.drv_rxbr_hline_rcv_cfg                 0x00015a0e   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    i.drv_rxbr_register_irq0_callback        0x00015a18   Section        0  drv_rxbr.o(i.drv_rxbr_register_irq0_callback)
    i.drv_rxbr_register_irq1_callback        0x00015a24   Section        0  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    i.drv_rxbr_set_ack_pkt_header            0x00015a30   Section        0  drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header)
    i.drv_rxbr_set_color_format              0x00015a44   Section        0  drv_rxbr.o(i.drv_rxbr_set_color_format)
    i.drv_rxbr_set_filter_regs               0x00015a58   Section        0  drv_rxbr.o(i.drv_rxbr_set_filter_regs)
    i.drv_rxbr_set_inten                     0x00015a6a   Section        0  drv_rxbr.o(i.drv_rxbr_set_inten)
    i.drv_rxbr_set_ltpo_drop_th              0x00015a7e   Section        0  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    i.drv_rxbr_set_usr_cfg                   0x00015a8e   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    i.drv_rxbr_set_usr_col                   0x00015ab4   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    i.drv_rxbr_set_usr_row                   0x00015abc   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    i.drv_swire_set_int                      0x00015ac4   Section        0  drv_swire.o(i.drv_swire_set_int)
    i.drv_sys_cfg_clear_all_int              0x00015b18   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    i.drv_sys_cfg_clear_pending              0x00015b24   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    i.drv_sys_cfg_sel_ap_rst_lvl_trig        0x00015b4c   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig)
    i.drv_sys_cfg_set_int                    0x00015b64   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    i.drv_timer_clear_status_flags           0x00015b88   Section        0  drv_timer.o(i.drv_timer_clear_status_flags)
    drv_timer_clear_status_flags             0x00015b89   Thumb Code    26  drv_timer.o(i.drv_timer_clear_status_flags)
    i.drv_timer_enable                       0x00015ba2   Section        0  drv_timer.o(i.drv_timer_enable)
    i.drv_timer_get_instance                 0x00015bc4   Section        0  drv_timer.o(i.drv_timer_get_instance)
    i.drv_timer_handle_interrupt             0x00015bd4   Section        0  drv_timer.o(i.drv_timer_handle_interrupt)
    drv_timer_handle_interrupt               0x00015bd5   Thumb Code    62  drv_timer.o(i.drv_timer_handle_interrupt)
    i.drv_timer_set_compare_val              0x00015c18   Section        0  drv_timer.o(i.drv_timer_set_compare_val)
    i.drv_timer_set_int                      0x00015c28   Section        0  drv_timer.o(i.drv_timer_set_int)
    i.drv_tx_phy_test_clear                  0x00015c7c   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_clear)
    drv_tx_phy_test_clear                    0x00015c7d   Thumb Code    10  drv_dsi_tx.o(i.drv_tx_phy_test_clear)
    i.drv_tx_phy_test_enter                  0x00015c86   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    i.drv_tx_phy_test_exit                   0x00015ca2   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    i.drv_tx_phy_test_write_1_byte           0x00015cbe   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte)
    drv_tx_phy_test_write_1_byte             0x00015cbf   Thumb Code    18  drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte)
    i.drv_tx_phy_test_write_2_byte           0x00015cd0   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte)
    drv_tx_phy_test_write_2_byte             0x00015cd1   Thumb Code    20  drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte)
    i.drv_tx_phy_test_write_code             0x00015ce4   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    drv_tx_phy_test_write_code               0x00015ce5   Thumb Code    16  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    i.drv_vidc_clear_irq                     0x00015cf4   Section        0  drv_vidc.o(i.drv_vidc_clear_irq)
    i.drv_vidc_enable                        0x00015cfc   Section        0  drv_vidc.o(i.drv_vidc_enable)
    i.drv_vidc_enable_irq                    0x00015d14   Section        0  drv_vidc.o(i.drv_vidc_enable_irq)
    i.drv_vidc_get_irq_status                0x00015d54   Section        0  drv_vidc.o(i.drv_vidc_get_irq_status)
    i.drv_vidc_init_module_enable            0x00015d68   Section        0  drv_vidc.o(i.drv_vidc_init_module_enable)
    i.drv_vidc_register_callback             0x00015d90   Section        0  drv_vidc.o(i.drv_vidc_register_callback)
    i.drv_vidc_reset                         0x00015d9c   Section        0  drv_vidc.o(i.drv_vidc_reset)
    i.drv_vidc_set_dst_parameter             0x00015da2   Section        0  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    i.drv_vidc_set_irqen                     0x00015dde   Section        0  drv_vidc.o(i.drv_vidc_set_irqen)
    i.drv_vidc_set_mirror                    0x00015df2   Section        0  drv_vidc.o(i.drv_vidc_set_mirror)
    i.drv_vidc_set_p2r_hcoef0                0x00015e02   Section        0  drv_vidc.o(i.drv_vidc_set_p2r_hcoef0)
    i.drv_vidc_set_p2r_hinitb                0x00015e0a   Section        0  drv_vidc.o(i.drv_vidc_set_p2r_hinitb)
    i.drv_vidc_set_p2r_hinitr                0x00015e30   Section        0  drv_vidc.o(i.drv_vidc_set_p2r_hinitr)
    i.drv_vidc_set_pentile_swap              0x00015e58   Section        0  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    i.drv_vidc_set_pu_ctrl                   0x00015e70   Section        0  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    i.drv_vidc_set_rotation                  0x00015e7a   Section        0  drv_vidc.o(i.drv_vidc_set_rotation)
    i.drv_vidc_set_scld_hcoef0               0x00015e8a   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    i.drv_vidc_set_scld_hcoef1               0x00015e94   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    i.drv_vidc_set_scld_step                 0x00015e9e   Section        0  drv_vidc.o(i.drv_vidc_set_scld_step)
    i.drv_vidc_set_scld_vcoef0               0x00015eb0   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    i.drv_vidc_set_scld_vcoef1               0x00015eba   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    i.drv_vidc_set_src_parameter             0x00015ec4   Section        0  drv_vidc.o(i.drv_vidc_set_src_parameter)
    i.drv_wdg_clear_counter                  0x00015edc   Section        0  drv_wdg.o(i.drv_wdg_clear_counter)
    i.drv_wdg_clear_edge_flag                0x00015eec   Section        0  drv_wdg.o(i.drv_wdg_clear_edge_flag)
    drv_wdg_clear_edge_flag                  0x00015eed   Thumb Code    12  drv_wdg.o(i.drv_wdg_clear_edge_flag)
    i.drv_wdg_read_edge_flag                 0x00015efc   Section        0  drv_wdg.o(i.drv_wdg_read_edge_flag)
    drv_wdg_read_edge_flag                   0x00015efd   Thumb Code    10  drv_wdg.o(i.drv_wdg_read_edge_flag)
    i.drv_wdg_set_int                        0x00015f0c   Section        0  drv_wdg.o(i.drv_wdg_set_int)
    i.fls_clr_interrupt_flag                 0x00015f4c   Section        0  drv_fls.o(i.fls_clr_interrupt_flag)
    i.fputc                                  0x00015f56   Section        0  tau_log.o(i.fputc)
    i.frame_start_cb                         0x00015f6c   Section        0  ap_demo.o(i.frame_start_cb)
    frame_start_cb                           0x00015f6d   Thumb Code    38  ap_demo.o(i.frame_start_cb)
    i.hal_dsi_rx_ctrl_create_handle          0x00015fbc   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    i.hal_dsi_rx_ctrl_dsc_async_handler      0x00015ff0   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler)
    i.hal_dsi_rx_ctrl_gen_a_tear_signal      0x00016018   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal)
    i.hal_dsi_rx_ctrl_get_max_ret_size       0x00016040   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size)
    i.hal_dsi_rx_ctrl_init                   0x00016068   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    i.hal_dsi_rx_ctrl_init_clk               0x00016100   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    hal_dsi_rx_ctrl_init_clk                 0x00016101   Thumb Code   332  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    i.hal_dsi_rx_ctrl_init_dsi_rx            0x000162a4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    hal_dsi_rx_ctrl_init_dsi_rx              0x000162a5   Thumb Code   184  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    i.hal_dsi_rx_ctrl_init_memc              0x0001637c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    hal_dsi_rx_ctrl_init_memc                0x0001637d   Thumb Code   342  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    i.hal_dsi_rx_ctrl_init_rxbr              0x000164dc   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    hal_dsi_rx_ctrl_init_rxbr                0x000164dd   Thumb Code   320  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    i.hal_dsi_rx_ctrl_init_vidc              0x0001662c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    hal_dsi_rx_ctrl_init_vidc                0x0001662d   Thumb Code   544  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    i.hal_dsi_rx_ctrl_pre_init_pps           0x00016858   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    i.hal_dsi_rx_ctrl_restart                0x00016894   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart)
    i.hal_dsi_rx_ctrl_send_ack_cmd           0x000168e4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd)
    i.hal_dsi_rx_ctrl_set_cus_esc_clk        0x000169d4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk)
    i.hal_dsi_rx_ctrl_set_cus_scld_filter    0x00016a00   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter)
    i.hal_dsi_rx_ctrl_set_cus_sync_line      0x00016a6c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line)
    i.hal_dsi_rx_ctrl_set_ipi_cfg            0x00016aa0   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    hal_dsi_rx_ctrl_set_ipi_cfg              0x00016aa1   Thumb Code    50  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    i.hal_dsi_rx_ctrl_set_rxbr_clk           0x00016ad8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk)
    hal_dsi_rx_ctrl_set_rxbr_clk             0x00016ad9   Thumb Code   114  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk)
    i.hal_dsi_rx_ctrl_set_tear_mode_ex       0x00016b4a   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex)
    i.hal_dsi_rx_ctrl_start                  0x00016b58   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    i.hal_dsi_rx_ctrl_toggle_resolution      0x00016b94   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    i.hal_dsi_tx_calc_video_chunks           0x00016bb4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks)
    hal_dsi_tx_calc_video_chunks             0x00016bb5   Thumb Code   384  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks)
    i.hal_dsi_tx_config_params_for_lane_rate 0x00016d44   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate)
    hal_dsi_tx_config_params_for_lane_rate   0x00016d45   Thumb Code    42  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate)
    i.hal_dsi_tx_count_lane_rate             0x00016d78   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate)
    hal_dsi_tx_count_lane_rate               0x00016d79   Thumb Code   982  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate)
    i.hal_dsi_tx_ctrl_create_handle          0x000171a0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    i.hal_dsi_tx_ctrl_enter_init_panel_mode  0x000171cc   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode)
    i.hal_dsi_tx_ctrl_exit_init_panel_mode   0x00017218   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode)
    i.hal_dsi_tx_ctrl_init                   0x00017240   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    i.hal_dsi_tx_ctrl_init_clk               0x000172e4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    hal_dsi_tx_ctrl_init_clk                 0x000172e5   Thumb Code    36  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    i.hal_dsi_tx_ctrl_panel_reset_pin        0x00017308   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin)
    i.hal_dsi_tx_ctrl_set_ccm                0x00017314   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm)
    i.hal_dsi_tx_ctrl_set_overwrite_rgb      0x00017334   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    i.hal_dsi_tx_ctrl_set_partial_disp       0x00017348   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp)
    i.hal_dsi_tx_ctrl_set_partial_disp_area  0x00017358   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area)
    i.hal_dsi_tx_ctrl_start                  0x0001737c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    i.hal_dsi_tx_ctrl_write_array_cmd        0x00017424   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd)
    i.hal_dsi_tx_ctrl_write_cmd              0x00017514   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    i.hal_dsi_tx_init_data_mode              0x000175e0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode)
    hal_dsi_tx_init_data_mode                0x000175e1   Thumb Code    58  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode)
    i.hal_dsi_tx_init_dpi_cfg                0x00017624   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg)
    hal_dsi_tx_init_dpi_cfg                  0x00017625   Thumb Code    42  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg)
    i.hal_dsi_tx_init_interrupt              0x00017654   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt)
    hal_dsi_tx_init_interrupt                0x00017655   Thumb Code    28  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt)
    i.hal_dsi_tx_init_phy_cfg                0x00017674   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    hal_dsi_tx_init_phy_cfg                  0x00017675   Thumb Code    28  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    i.hal_dsi_tx_init_remains                0x00017694   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains)
    hal_dsi_tx_init_remains                  0x00017695   Thumb Code   142  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains)
    i.hal_dsi_tx_init_video_mode             0x00017728   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode)
    hal_dsi_tx_init_video_mode               0x00017729   Thumb Code    82  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode)
    i.hal_dsi_tx_send_cmd                    0x00017780   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    hal_dsi_tx_send_cmd                      0x00017781   Thumb Code    60  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    i.hal_gpio_init_output                   0x000177c4   Section        0  hal_gpio.o(i.hal_gpio_init_output)
    i.hal_gpio_set_mode                      0x000177ec   Section        0  hal_gpio.o(i.hal_gpio_set_mode)
    i.hal_gpio_set_output_data               0x0001784c   Section        0  hal_gpio.o(i.hal_gpio_set_output_data)
    i.hal_internal_check_video_auto_sync     0x00017854   Section        0  hal_internal_vsync.o(i.hal_internal_check_video_auto_sync)
    i.hal_internal_init_memc                 0x0001786c   Section        0  hal_internal_vsync.o(i.hal_internal_init_memc)
    i.hal_internal_rx_dcs_async_handler      0x00017968   Section        0  hal_internal_vsync.o(i.hal_internal_rx_dcs_async_handler)
    i.hal_internal_rx_dcs_polling            0x00017994   Section        0  hal_internal_vsync.o(i.hal_internal_rx_dcs_polling)
    i.hal_internal_sync_get_fb_setting       0x000179ec   Section        0  hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting)
    i.hal_internal_sync_get_hight_performan_mode 0x000179fc   Section        0  hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode)
    i.hal_internal_sync_input_resolution_change 0x00017a0c   Section        0  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    i.hal_internal_vsync_deinit              0x00017c38   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    i.hal_internal_vsync_get_sync_line       0x00017c60   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    i.hal_internal_vsync_get_tear_mode       0x00017c78   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_tear_mode)
    i.hal_internal_vsync_get_tx_state        0x00017c84   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    i.hal_internal_vsync_init_rx             0x00017c90   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    i.hal_internal_vsync_init_tx             0x00017dd0   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    i.hal_internal_vsync_set_auto_hw_filter  0x00017e80   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter)
    i.hal_internal_vsync_set_rx_state        0x00017f10   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    i.hal_internal_vsync_set_sync_line       0x00017f34   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line)
    i.hal_internal_vsync_set_tear_mode       0x00017f78   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    i.hal_internal_vsync_set_tx_state        0x00017fc8   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    i.hal_intl_svs_deinit_tx                 0x0001804c   Section        0  hal_internal_soft_sync.o(i.hal_intl_svs_deinit_tx)
    i.hal_intl_svs_handle                    0x0001805c   Section        0  hal_internal_soft_sync.o(i.hal_intl_svs_handle)
    i.hal_intl_svs_init_rx                   0x00018080   Section        0  hal_internal_soft_sync.o(i.hal_intl_svs_init_rx)
    i.hal_intl_svs_init_tx                   0x000180f8   Section        0  hal_internal_soft_sync.o(i.hal_intl_svs_init_tx)
    i.hal_intl_svs_set_sync_coef             0x0001810c   Section        0  hal_internal_soft_sync.o(i.hal_intl_svs_set_sync_coef)
    i.hal_intl_svs_update_rxbr_clk           0x00018118   Section        0  hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk)
    i.hal_lcdc_config_ccm                    0x00018160   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm)
    hal_lcdc_config_ccm                      0x00018161   Thumb Code    30  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm)
    i.hal_lcdc_config_remains                0x00018184   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains)
    hal_lcdc_config_remains                  0x00018185   Thumb Code    94  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains)
    i.hal_lcdc_config_rgb_to_pentile         0x000181e8   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile)
    hal_lcdc_config_rgb_to_pentile           0x000181e9   Thumb Code    14  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile)
    i.hal_lcdc_config_upscaler               0x000181fc   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler)
    hal_lcdc_config_upscaler                 0x000181fd   Thumb Code   348  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler)
    i.hal_lcdc_init_cfg                      0x00018360   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    hal_lcdc_init_cfg                        0x00018361   Thumb Code    78  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    i.hal_lcdc_init_clk                      0x000183b4   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    hal_lcdc_init_clk                        0x000183b5   Thumb Code   446  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    i.hal_lcdc_init_interrupt                0x00018580   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt)
    hal_lcdc_init_interrupt                  0x00018581   Thumb Code    58  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt)
    i.hal_system_enable_systick              0x000185c0   Section        0  hal_system.o(i.hal_system_enable_systick)
    i.hal_system_init                        0x000185c8   Section        0  hal_system.o(i.hal_system_init)
    i.hal_system_init_console                0x00018650   Section        0  hal_system.o(i.hal_system_init_console)
    i.hal_system_set_phy_calibration         0x0001866c   Section        0  hal_system.o(i.hal_system_set_phy_calibration)
    i.hal_tx_frame_rate_adjust               0x00018674   Section        0  hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust)
    hal_tx_frame_rate_adjust                 0x00018675   Thumb Code    44  hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust)
    i.hal_uart_init                          0x000186a4   Section        0  hal_uart.o(i.hal_uart_init)
    i.hal_uart_transmit_blocking             0x00018730   Section        0  hal_uart.o(i.hal_uart_transmit_blocking)
    i.handle_init                            0x00018740   Section        0  irq_redirect .o(i.handle_init)
    i.init_mipi_tx                           0x00018850   Section        0  ap_demo.o(i.init_mipi_tx)
    init_mipi_tx                             0x00018851   Thumb Code   100  ap_demo.o(i.init_mipi_tx)
    i.init_panel                             0x000188bc   Section        0  ap_demo.o(i.init_panel)
    init_panel                               0x000188bd   Thumb Code   150  ap_demo.o(i.init_panel)
    i.main                                   0x0001895c   Section        0  main.o(i.main)
    i.open_mipi_rx                           0x00018968   Section        0  ap_demo.o(i.open_mipi_rx)
    open_mipi_rx                             0x00018969   Thumb Code   170  ap_demo.o(i.open_mipi_rx)
    i.pps_update_handle                      0x00018a3c   Section        0  ap_demo.o(i.pps_update_handle)
    pps_update_handle                        0x00018a3d   Thumb Code    78  ap_demo.o(i.pps_update_handle)
    i.rx_get_dcs_packet_data                 0x00018ad8   Section        0  hal_internal_vsync.o(i.rx_get_dcs_packet_data)
    rx_get_dcs_packet_data                   0x00018ad9   Thumb Code   654  hal_internal_vsync.o(i.rx_get_dcs_packet_data)
    i.rx_partial_update                      0x00018ecc   Section        0  hal_internal_vsync.o(i.rx_partial_update)
    rx_partial_update                        0x00018ecd   Thumb Code   348  hal_internal_vsync.o(i.rx_partial_update)
    i.rx_receive_packet                      0x00019038   Section        0  hal_internal_vsync.o(i.rx_receive_packet)
    rx_receive_packet                        0x00019039   Thumb Code   126  hal_internal_vsync.o(i.rx_receive_packet)
    i.rx_receive_pps                         0x000190c4   Section        0  hal_internal_vsync.o(i.rx_receive_pps)
    rx_receive_pps                           0x000190c5   Thumb Code   268  hal_internal_vsync.o(i.rx_receive_pps)
    i.rxbr_irq0_callback                     0x00019244   Section        0  hal_internal_vsync.o(i.rxbr_irq0_callback)
    rxbr_irq0_callback                       0x00019245   Thumb Code   192  hal_internal_vsync.o(i.rxbr_irq0_callback)
    i.rxbr_irq1_callback                     0x00019310   Section        0  hal_internal_vsync.o(i.rxbr_irq1_callback)
    rxbr_irq1_callback                       0x00019311   Thumb Code   392  hal_internal_vsync.o(i.rxbr_irq1_callback)
    i.soft_gen_te                            0x00019554   Section        0  hal_internal_vsync.o(i.soft_gen_te)
    soft_gen_te                              0x00019555   Thumb Code   166  hal_internal_vsync.o(i.soft_gen_te)
    i.soft_gen_te_double_buffer              0x00019618   Section        0  hal_internal_vsync.o(i.soft_gen_te_double_buffer)
    soft_gen_te_double_buffer                0x00019619   Thumb Code   166  hal_internal_vsync.o(i.soft_gen_te_double_buffer)
    i.sqrt                                   0x000196d8   Section        0  sqrt.o(i.sqrt)
    i.svs_direct_mode_setting                0x00019720   Section        0  hal_internal_soft_sync.o(i.svs_direct_mode_setting)
    svs_direct_mode_setting                  0x00019721   Thumb Code   156  hal_internal_soft_sync.o(i.svs_direct_mode_setting)
    i.svs_get_rel_intv                       0x000197cc   Section        0  hal_internal_soft_sync.o(i.svs_get_rel_intv)
    svs_get_rel_intv                         0x000197cd   Thumb Code    20  hal_internal_soft_sync.o(i.svs_get_rel_intv)
    i.svs_sync_handle                        0x000197e8   Section        0  hal_internal_soft_sync.o(i.svs_sync_handle)
    svs_sync_handle                          0x000197e9   Thumb Code   158  hal_internal_soft_sync.o(i.svs_sync_handle)
    i.svs_wait_start                         0x00019898   Section        0  hal_internal_soft_sync.o(i.svs_wait_start)
    svs_wait_start                           0x00019899   Thumb Code   224  hal_internal_soft_sync.o(i.svs_wait_start)
    i.svs_waite_fr_stab                      0x0001998c   Section        0  hal_internal_soft_sync.o(i.svs_waite_fr_stab)
    svs_waite_fr_stab                        0x0001998d   Thumb Code   148  hal_internal_soft_sync.o(i.svs_waite_fr_stab)
    i.vidc_callback                          0x00019a64   Section        0  hal_internal_vsync.o(i.vidc_callback)
    vidc_callback                            0x00019a65   Thumb Code   234  hal_internal_vsync.o(i.vidc_callback)
    i.vpre_err_reset                         0x00019b6c   Section        0  hal_internal_vsync.o(i.vpre_err_reset)
    vpre_err_reset                           0x00019b6d   Thumb Code   192  hal_internal_vsync.o(i.vpre_err_reset)
    i.vsync_set_te_mode                      0x00019c44   Section        0  hal_internal_vsync.o(i.vsync_set_te_mode)
    vsync_set_te_mode                        0x00019c45   Thumb Code   300  hal_internal_vsync.o(i.vsync_set_te_mode)
    .constdata                               0x00019e10   Section     8052  ap_demo.o(.constdata)
    g_cus_rx_dcs_execute_table               0x00019e10   Data         108  ap_demo.o(.constdata)
    .constdata                               0x0001bd84   Section      210  hal_gpio.o(.constdata)
    s_gpio_map                               0x0001bd84   Data         120  hal_gpio.o(.constdata)
    s_gpio_perf                              0x0001bdfc   Data          90  hal_gpio.o(.constdata)
    .constdata                               0x0001be58   Section        8  drv_param_init.o(.constdata)
    .constdata                               0x0001be60   Section      390  drv_phy_common.o(.constdata)
    phy_para_mapping_h                       0x0001be60   Data         184  drv_phy_common.o(.constdata)
    phy_para_mapping_l                       0x0001bf18   Data         128  drv_phy_common.o(.constdata)
    phy_data_high_map                        0x0001bf98   Data          48  drv_phy_common.o(.constdata)
    phy_data_lp_map                          0x0001bfc8   Data          30  drv_phy_common.o(.constdata)
    .conststring                             0x0001bfe8   Section       72  hal_dsi_rx_ctrl.o(.conststring)
    .conststring                             0x0001c030   Section       67  hal_dsi_tx_ctrl.o(.conststring)
    .conststring                             0x0001c074   Section      376  hal_internal_vsync.o(.conststring)
    .ARM.__AT_0x00070100                     0x00070100   Section      192  irq_redirect .o(.ARM.__AT_0x00070100)
    .data                                    0x000701d0   Section      560  ap_demo.o(.data)
    start_display_on                         0x000701d0   Data           1  ap_demo.o(.data)
    g_exit_sleep_mode                        0x000701d1   Data           1  ap_demo.o(.data)
    S21_G991B_frame_update                   0x000701d2   Data           1  ap_demo.o(.data)
    s_in_aod_mode_flag                       0x000701d3   Data           1  ap_demo.o(.data)
    s_in_bule_mode_flag                      0x000701d4   Data           1  ap_demo.o(.data)
    panel_display_done                       0x000701d5   Data           1  ap_demo.o(.data)
    isStart                                  0x000701d6   Data           1  ap_demo.o(.data)
    flag_0a                                  0x000701d9   Data           1  ap_demo.o(.data)
    flag_5a                                  0x000701da   Data           1  ap_demo.o(.data)
    flag_c9_43                               0x000701db   Data           1  ap_demo.o(.data)
    ret_7f_count                             0x000701dc   Data           1  ap_demo.o(.data)
    ret_a1_count                             0x000701dd   Data           1  ap_demo.o(.data)
    ret_a2_count                             0x000701de   Data           1  ap_demo.o(.data)
    ret_c6_count                             0x000701df   Data           1  ap_demo.o(.data)
    ret_c7_count                             0x000701e0   Data           1  ap_demo.o(.data)
    ret_c8_count                             0x000701e1   Data           1  ap_demo.o(.data)
    ret_c9_count                             0x000701e2   Data           1  ap_demo.o(.data)
    frame_rate                               0x000701e3   Data           1  ap_demo.o(.data)
    g_rx_ctrl_handle                         0x000701ec   Data           4  ap_demo.o(.data)
    g_tx_ctrl_handle                         0x000701f0   Data           4  ap_demo.o(.data)
    curFrame                                 0x000701f4   Data           4  ap_demo.o(.data)
    value_reg_df                             0x000701fc   Data           4  ap_demo.o(.data)
    .data                                    0x00070400   Section       59  app_tp_st_touch.o(.data)
    s_calibration_flag                       0x00070403   Data           1  app_tp_st_touch.o(.data)
    s_calibration_correct_flag               0x00070404   Data           1  app_tp_st_touch.o(.data)
    .data                                    0x0007043c   Section      228  app_tp_for_custom_s8.o(.data)
    app_tp_count                             0x00070446   Data           1  app_tp_for_custom_s8.o(.data)
    phone_85_flag                            0x00070447   Data           1  app_tp_for_custom_s8.o(.data)
    phone_F6_flag                            0x00070448   Data           1  app_tp_for_custom_s8.o(.data)
    phone_E4_flag                            0x00070449   Data           1  app_tp_for_custom_s8.o(.data)
    phone_72_flag                            0x0007044a   Data           1  app_tp_for_custom_s8.o(.data)
    phone_75_flag                            0x0007044b   Data           1  app_tp_for_custom_s8.o(.data)
    phone_92_flag                            0x0007044c   Data           1  app_tp_for_custom_s8.o(.data)
    phone_74_flag                            0x0007044d   Data           1  app_tp_for_custom_s8.o(.data)
    u16CoordY                                0x00070450   Data           2  app_tp_for_custom_s8.o(.data)
    u16CoordX                                0x00070452   Data           2  app_tp_for_custom_s8.o(.data)
    u16CoordY_back                           0x00070454   Data           2  app_tp_for_custom_s8.o(.data)
    u16CoordX_back                           0x00070456   Data           2  app_tp_for_custom_s8.o(.data)
    .data                                    0x00070520   Section        8  hal_dsi_rx_ctrl.o(.data)
    g_hw_auto_filter                         0x00070520   Data           1  hal_dsi_rx_ctrl.o(.data)
    g_esc_clk                                0x00070524   Data           4  hal_dsi_rx_ctrl.o(.data)
    .data                                    0x00070528   Section        3  hal_dsi_tx_ctrl.o(.data)
    g_tx_vcom_en                             0x00070528   Data           1  hal_dsi_tx_ctrl.o(.data)
    g_tx_vpg_en                              0x00070529   Data           1  hal_dsi_tx_ctrl.o(.data)
    g_tx_mode                                0x0007052a   Data           1  hal_dsi_tx_ctrl.o(.data)
    .data                                    0x0007052c   Section       24  hal_internal_vsync.o(.data)
    sg_cmd_mode_tx_start                     0x0007052c   Data           1  hal_internal_vsync.o(.data)
    sg_cur_te_info                           0x00070530   Data           4  hal_internal_vsync.o(.data)
    g_cus_rx_write_cmd_handle                0x00070538   Data          12  hal_internal_vsync.o(.data)
    .data                                    0x00070544   Section       12  drv_common.o(.data)
    s_my_tick                                0x00070544   Data           4  drv_common.o(.data)
    .data                                    0x00070550   Section        4  drv_gpio.o(.data)
    g_ap_reset_cb                            0x00070550   Data           4  drv_gpio.o(.data)
    .data                                    0x00070554   Section        4  drv_i2c_master.o(.data)
    i2c1_intr_callback                       0x00070554   Data           4  drv_i2c_master.o(.data)
    .data                                    0x00070558   Section        4  drv_i2c_slave.o(.data)
    i2c0_intr_callback                       0x00070558   Data           4  drv_i2c_slave.o(.data)
    .data                                    0x0007055c   Section     1188  drv_param_init.o(.data)
    .data                                    0x00070a00   Section        4  drv_spi_master.o(.data)
    SPIM_intr_callback                       0x00070a00   Data           4  drv_spi_master.o(.data)
    .data                                    0x00070a04   Section        1  drv_sys_cfg.o(.data)
    sg_ap_rstn_trigger_type                  0x00070a04   Data           1  drv_sys_cfg.o(.data)
    .data                                    0x00070a08   Section        8  drv_rxbr.o(.data)
    .data                                    0x00070a10   Section        4  drv_vidc.o(.data)
    .data                                    0x00070a14   Section        1  drv_phy_common.o(.data)
    g_phy_calibration                        0x00070a14   Data           1  drv_phy_common.o(.data)
    .data                                    0x00070a18   Section       12  drv_chip_info.o(.data)
    sg_chip_info                             0x00070a18   Data           4  drv_chip_info.o(.data)
    sg_chip_function                         0x00070a1c   Data           4  drv_chip_info.o(.data)
    sg_chip_encrypt                          0x00070a20   Data           4  drv_chip_info.o(.data)
    .data                                    0x00070a24   Section       18  norflash.o(.data)
    tmprg                                    0x00070a2c   Data           4  norflash.o(.data)
    .data                                    0x00070a38   Section       12  drv_pwm.o(.data)
    s_pwm_type                               0x00070a38   Data           1  drv_pwm.o(.data)
    s_pwm_cb                                 0x00070a3c   Data           8  drv_pwm.o(.data)
    .data                                    0x00070a44   Section        8  drv_swire.o(.data)
    s_swire_cb                               0x00070a44   Data           8  drv_swire.o(.data)
    .data                                    0x00070a4c   Section       80  drv_timer.o(.data)
    sg_timer_info                            0x00070a4c   Data          80  drv_timer.o(.data)
    .data                                    0x00070a9c   Section        8  drv_uart.o(.data)
    s_UartFcrReg                             0x00070a9c   Data           4  drv_uart.o(.data)
    uart_userData                            0x00070aa0   Data           4  drv_uart.o(.data)
    .data                                    0x00070aa4   Section       12  drv_wdg.o(.data)
    sg_wdg_repeat                            0x00070aa4   Data           1  drv_wdg.o(.data)
    sg_wdg_cb                                0x00070aa8   Data           8  drv_wdg.o(.data)
    .data                                    0x00070ab0   Section        4  stdout.o(.data)
    .data                                    0x00070ab4   Section        4  errno.o(.data)
    _errno                                   0x00070ab4   Data           4  errno.o(.data)
    .bss                                     0x00070ab8   Section       36  ap_demo.o(.bss)
    ccm                                      0x00070ab8   Data          36  ap_demo.o(.bss)
    .bss                                     0x00070adc   Section      196  hal_dsi_rx_ctrl.o(.bss)
    g_rx_ctrl_handle_inst                    0x00070adc   Data         196  hal_dsi_rx_ctrl.o(.bss)
    .bss                                     0x00070ba0   Section       76  hal_dsi_tx_ctrl.o(.bss)
    g_tx_ctrl_handle_inst                    0x00070ba0   Data          76  hal_dsi_tx_ctrl.o(.bss)
    .bss                                     0x00070bec   Section      256  tau_log.o(.bss)
    .bss                                     0x00070cec   Section      208  hal_uart.o(.bss)
    .bss                                     0x00070dbc   Section     2420  hal_internal_vsync.o(.bss)
    g_imm_buffer                             0x00071610   Data         255  hal_internal_vsync.o(.bss)
    sg_te_info                               0x00071710   Data          12  hal_internal_vsync.o(.bss)
    g_imm_packet                             0x0007171c   Data          20  hal_internal_vsync.o(.bss)
    .bss                                     0x00071730   Section       28  drv_dma.o(.bss)
    s_dma_handle                             0x00071730   Data          28  drv_dma.o(.bss)
    .bss                                     0x0007174c   Section       64  drv_gpio.o(.bss)
    s_gpio_cb                                0x0007174c   Data          64  drv_gpio.o(.bss)
    .bss                                     0x0007178c   Section       64  hal_internal_soft_sync.o(.bss)
    sg_sys_handler                           0x0007178c   Data          64  hal_internal_soft_sync.o(.bss)
    .bss                                     0x000717cc   Section       32  hal_spi_slave.o(.bss)
    .bss                                     0x000717ec   Section     4144  dcs_packet_fifo.o(.bss)
    STACK                                    0x00072820   Section     4096  startup_armcm0.o(STACK)

    Global Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    BuildAttributes$$THM_ISAv3M$S$PE$A:L22$X:L11$S22$IEEE1$IW$USESV6$~STKCKD$USESV7$~SHL$OTIME$ROPI$IEEEJ$EBA8$MICROLIB$REQ8$PRES8$EABIv2 0x00000000   Number         0  anon$$obj.o ABSOLUTE
    __ARM_use_no_argv                        0x00000000   Number         0  main.o ABSOLUTE
    _printf_a                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_c                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_charcount                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_d                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_e                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_f                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_flags                            0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_dec                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_hex                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_g                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_i                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_int_dec                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_l                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ll                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lld                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lli                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llo                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llu                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llx                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_dec                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_hex                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_oct                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ls                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_mbtowc                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_n                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_o                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_p                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_percent                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_pre_padding                      0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_return_value                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_s                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_sizespec                         0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_str                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_signed                  0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_unsigned                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_u                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wctomb                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_widthprec                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_x                                0x00000000   Number         0  stubs.o ABSOLUTE
    __cpp_initialize__aeabi_                  - Undefined Weak Reference
    __cxa_finalize                            - Undefined Weak Reference
    _clock_init                               - Undefined Weak Reference
    _microlib_exit                            - Undefined Weak Reference
    __Vectors_Size                           0x000000c0   Number         0  startup_armcm0.o ABSOLUTE
    __Vectors                                0x00010000   Data           4  startup_armcm0.o(RESET)
    __Vectors_End                            0x000100c0   Data           0  startup_armcm0.o(RESET)
    __main                                   0x000100c1   Thumb Code     0  entry.o(.ARM.Collect$$$$00000000)
    _main_stk                                0x000100c1   Thumb Code     0  entry2.o(.ARM.Collect$$$$00000001)
    _main_scatterload                        0x000100c5   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    __main_after_scatterload                 0x000100c9   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    _main_clock                              0x000100c9   Thumb Code     0  entry7b.o(.ARM.Collect$$$$00000008)
    _main_cpp_init                           0x000100c9   Thumb Code     0  entry8b.o(.ARM.Collect$$$$0000000A)
    _main_init                               0x000100c9   Thumb Code     0  entry9a.o(.ARM.Collect$$$$0000000B)
    __rt_final_cpp                           0x000100d1   Thumb Code     0  entry10a.o(.ARM.Collect$$$$0000000D)
    __rt_final_exit                          0x000100d1   Thumb Code     0  entry11a.o(.ARM.Collect$$$$0000000F)
    Reset_Handler                            0x000100d5   Thumb Code    28  startup_armcm0.o(.text)
    NMI_Handler                              0x000100f1   Thumb Code     2  startup_armcm0.o(.text)
    SVC_Handler                              0x000100f5   Thumb Code     2  startup_armcm0.o(.text)
    PendSV_Handler                           0x000100f7   Thumb Code     2  startup_armcm0.o(.text)
    OTP_IRQn_Handler                         0x00010123   Thumb Code     2  startup_armcm0.o(.text)
    PVD_IRQn_Handler                         0x00010127   Thumb Code     2  startup_armcm0.o(.text)
    __aeabi_uidiv                            0x0001014d   Thumb Code     0  uidiv.o(.text)
    __aeabi_uidivmod                         0x0001014d   Thumb Code    44  uidiv.o(.text)
    __aeabi_idiv                             0x00010179   Thumb Code     0  idiv.o(.text)
    __aeabi_idivmod                          0x00010179   Thumb Code    40  idiv.o(.text)
    __aeabi_memcpy                           0x000101a1   Thumb Code    36  memcpya.o(.text)
    __aeabi_memcpy4                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memcpy8                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memset                           0x000101c5   Thumb Code    14  memseta.o(.text)
    __aeabi_memset4                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memset8                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr                           0x000101d3   Thumb Code     4  memseta.o(.text)
    __aeabi_memclr4                          0x000101d3   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr8                          0x000101d3   Thumb Code     0  memseta.o(.text)
    _memset$wrapper                          0x000101d7   Thumb Code    18  memseta.o(.text)
    __aeabi_fadd                             0x000101e9   Thumb Code   162  fadd.o(.text)
    __aeabi_fsub                             0x0001028b   Thumb Code     8  fadd.o(.text)
    __aeabi_frsub                            0x00010293   Thumb Code     8  fadd.o(.text)
    __aeabi_fmul                             0x0001029b   Thumb Code   122  fmul.o(.text)
    __aeabi_fdiv                             0x00010315   Thumb Code   124  fdiv.o(.text)
    __ARM_scalbnf                            0x00010391   Thumb Code    24  fscalb.o(.text)
    scalbnf                                  0x00010391   Thumb Code     0  fscalb.o(.text)
    __aeabi_dadd                             0x000103a9   Thumb Code   328  dadd.o(.text)
    __aeabi_dsub                             0x000104f1   Thumb Code    12  dadd.o(.text)
    __aeabi_drsub                            0x000104fd   Thumb Code    12  dadd.o(.text)
    __aeabi_dmul                             0x0001050d   Thumb Code   202  dmul.o(.text)
    __aeabi_ddiv                             0x000105dd   Thumb Code   234  ddiv.o(.text)
    __aeabi_i2f                              0x000106cd   Thumb Code    22  fflti.o(.text)
    __aeabi_ui2f                             0x000106e3   Thumb Code    14  ffltui.o(.text)
    __aeabi_ui2d                             0x000106f1   Thumb Code    24  dfltui.o(.text)
    __aeabi_f2iz                             0x0001070d   Thumb Code    50  ffixi.o(.text)
    __aeabi_f2uiz                            0x0001073f   Thumb Code    40  ffixui.o(.text)
    __aeabi_d2iz                             0x00010769   Thumb Code    62  dfixi.o(.text)
    __aeabi_d2uiz                            0x000107b1   Thumb Code    50  dfixui.o(.text)
    __aeabi_f2d                              0x000107ed   Thumb Code    40  f2d.o(.text)
    __aeabi_cdcmpeq                          0x00010815   Thumb Code     0  cdcmple.o(.text)
    __aeabi_cdcmple                          0x00010815   Thumb Code    38  cdcmple.o(.text)
    __aeabi_cfcmpeq                          0x0001083d   Thumb Code     0  cfcmple.o(.text)
    __aeabi_cfcmple                          0x0001083d   Thumb Code    20  cfcmple.o(.text)
    __aeabi_cfrcmple                         0x00010851   Thumb Code    20  cfrcmple.o(.text)
    __aeabi_uldivmod                         0x00010865   Thumb Code    96  uldiv.o(.text)
    __aeabi_llsl                             0x000108c5   Thumb Code    32  llshl.o(.text)
    _ll_shift_l                              0x000108c5   Thumb Code     0  llshl.o(.text)
    __aeabi_llsr                             0x000108e5   Thumb Code    34  llushr.o(.text)
    _ll_ushift_r                             0x000108e5   Thumb Code     0  llushr.o(.text)
    __aeabi_lasr                             0x00010907   Thumb Code    38  llsshr.o(.text)
    _ll_sshift_r                             0x00010907   Thumb Code     0  llsshr.o(.text)
    __I$use$fp                               0x0001092d   Thumb Code     0  iusefp.o(.text)
    _float_round                             0x0001092d   Thumb Code    16  fepilogue.o(.text)
    _float_epilogue                          0x0001093d   Thumb Code   114  fepilogue.o(.text)
    _double_round                            0x000109af   Thumb Code    26  depilogue.o(.text)
    _double_epilogue                         0x000109c9   Thumb Code   164  depilogue.o(.text)
    _dsqrt                                   0x00010a6d   Thumb Code   162  dsqrt.o(.text)
    __aeabi_d2ulz                            0x00010b11   Thumb Code    54  dfixul.o(.text)
    __aeabi_cdrcmple                         0x00010b51   Thumb Code    38  cdrcmple.o(.text)
    __scatterload                            0x00010b79   Thumb Code    28  init.o(.text)
    __scatterload_rt2                        0x00010b79   Thumb Code     0  init.o(.text)
    __decompress                             0x00010b9d   Thumb Code     0  __dczerorl2.o(.text)
    __decompress1                            0x00010b9d   Thumb Code    86  __dczerorl2.o(.text)
    ADC_IRQn_Handler                         0x00010bf5   Thumb Code    18  irq_redirect .o(i.ADC_IRQn_Handler)
    AP_NRESET_IRQn_Handler                   0x00010c0d   Thumb Code    18  irq_redirect .o(i.AP_NRESET_IRQn_Handler)
    DMA_IRQn_Handler                         0x00010c25   Thumb Code    14  irq_redirect .o(i.DMA_IRQn_Handler)
    EXTI_INT0_IRQn_Handler                   0x00010c39   Thumb Code    22  irq_redirect .o(i.EXTI_INT0_IRQn_Handler)
    EXTI_INT1_IRQn_Handler                   0x00010c55   Thumb Code    22  irq_redirect .o(i.EXTI_INT1_IRQn_Handler)
    EXTI_INT2_IRQn_Handler                   0x00010c71   Thumb Code    22  irq_redirect .o(i.EXTI_INT2_IRQn_Handler)
    EXTI_INT3_IRQn_Handler                   0x00010c8d   Thumb Code    22  irq_redirect .o(i.EXTI_INT3_IRQn_Handler)
    EXTI_INT4_IRQn_Handler                   0x00010ca9   Thumb Code    22  irq_redirect .o(i.EXTI_INT4_IRQn_Handler)
    EXTI_INT5_IRQn_Handler                   0x00010cc5   Thumb Code    22  irq_redirect .o(i.EXTI_INT5_IRQn_Handler)
    EXTI_INT6_IRQn_Handler                   0x00010ce1   Thumb Code    22  irq_redirect .o(i.EXTI_INT6_IRQn_Handler)
    EXTI_INT7_IRQn_Handler                   0x00010cfd   Thumb Code    22  irq_redirect .o(i.EXTI_INT7_IRQn_Handler)
    FLSCTRL_IRQn_Handler                     0x00010d19   Thumb Code    14  irq_redirect .o(i.FLSCTRL_IRQn_Handler)
    Gpio_swire_output                        0x00010d2d   Thumb Code    78  ap_demo.o(i.Gpio_swire_output)
    HardFault_Handler                        0x00010d7d   Thumb Code    14  irq_redirect .o(i.HardFault_Handler)
    I2C0_IRQn_Handler                        0x00010d91   Thumb Code    18  irq_redirect .o(i.I2C0_IRQn_Handler)
    I2C1_IRQn_Handler                        0x00010da9   Thumb Code    18  irq_redirect .o(i.I2C1_IRQn_Handler)
    LCDC_IRQn_Handler                        0x00010dc1   Thumb Code    18  irq_redirect .o(i.LCDC_IRQn_Handler)
    LOG_printf                               0x00010dd9   Thumb Code    30  tau_log.o(i.LOG_printf)
    MEMC_IRQn_Handler                        0x00010e01   Thumb Code    18  irq_redirect .o(i.MEMC_IRQn_Handler)
    MIPI_RX_IRQn_Handler                     0x00010e19   Thumb Code    18  irq_redirect .o(i.MIPI_RX_IRQn_Handler)
    MIPI_TX_IRQn_Handler                     0x00010e31   Thumb Code    18  irq_redirect .o(i.MIPI_TX_IRQn_Handler)
    PWMDET_IRQn_Handler                      0x00010e49   Thumb Code    22  irq_redirect .o(i.PWMDET_IRQn_Handler)
    SPIM_IRQn_Handler                        0x00010e65   Thumb Code    22  irq_redirect .o(i.SPIM_IRQn_Handler)
    SPIS_IRQn_Handler                        0x00010e81   Thumb Code    22  irq_redirect .o(i.SPIS_IRQn_Handler)
    SWIRE_IRQn_Handler                       0x00010e9d   Thumb Code    22  irq_redirect .o(i.SWIRE_IRQn_Handler)
    SysTick_Handler                          0x00010eb9   Thumb Code    18  irq_redirect .o(i.SysTick_Handler)
    TIMER0_IRQn_Handler                      0x00010ed1   Thumb Code    18  irq_redirect .o(i.TIMER0_IRQn_Handler)
    TIMER1_IRQn_Handler                      0x00010ee9   Thumb Code    18  irq_redirect .o(i.TIMER1_IRQn_Handler)
    TIMER2_IRQn_Handler                      0x00010f01   Thumb Code    18  irq_redirect .o(i.TIMER2_IRQn_Handler)
    TIMER3_IRQn_Handler                      0x00010f19   Thumb Code    18  irq_redirect .o(i.TIMER3_IRQn_Handler)
    UART0_IRQ_Handle                         0x00010f31   Thumb Code    20  drv_uart.o(i.UART0_IRQ_Handle)
    UART_DisableDma                          0x00010f4d   Thumb Code     2  drv_uart.o(i.UART_DisableDma)
    UART_GetInstance                         0x00010f4f   Thumb Code     4  drv_uart.o(i.UART_GetInstance)
    UART_IRQn_Handler                        0x00010f55   Thumb Code    18  irq_redirect .o(i.UART_IRQn_Handler)
    UART_ResetRxFIFO                         0x00010f6d   Thumb Code    32  drv_uart.o(i.UART_ResetRxFIFO)
    UART_SetBaudRate                         0x00010f91   Thumb Code    72  drv_uart.o(i.UART_SetBaudRate)
    UART_SwitchSCLK                          0x00010fd9   Thumb Code    26  drv_uart.o(i.UART_SwitchSCLK)
    __scatterload_copy                       0x00010ff3   Thumb Code    14  handlers.o(i.__scatterload_copy)
    s_RAM_CK                                 0x00011000   Data          20  drv_common.o(.ARM.__at_0x11000)
    __scatterload_null                       0x00011015   Thumb Code     2  handlers.o(i.__scatterload_null)
    s_debug_state                            0x00011018   Data           4  drv_common.o(.ARM.__at_0x11018)
    UART_TransferHandleIRQ                   0x0001101d   Thumb Code   308  drv_uart.o(i.UART_TransferHandleIRQ)
    UART_WriteBlocking                       0x00011151   Thumb Code    26  drv_uart.o(i.UART_WriteBlocking)
    UART_init                                0x0001116d   Thumb Code   182  drv_uart.o(i.UART_init)
    VIDC_IRQn_Handler                        0x00011229   Thumb Code    18  irq_redirect .o(i.VIDC_IRQn_Handler)
    VPRE_IRQn_Handler                        0x00011241   Thumb Code    18  irq_redirect .o(i.VPRE_IRQn_Handler)
    WDG_IRQn_Handler                         0x00011259   Thumb Code    18  irq_redirect .o(i.WDG_IRQn_Handler)
    __0printf                                0x00011271   Thumb Code    24  printfa.o(i.__0printf)
    __1printf                                0x00011271   Thumb Code     0  printfa.o(i.__0printf)
    __2printf                                0x00011271   Thumb Code     0  printfa.o(i.__0printf)
    __c89printf                              0x00011271   Thumb Code     0  printfa.o(i.__0printf)
    printf                                   0x00011271   Thumb Code     0  printfa.o(i.__0printf)
    __0vsprintf                              0x00011291   Thumb Code    30  printfa.o(i.__0vsprintf)
    __1vsprintf                              0x00011291   Thumb Code     0  printfa.o(i.__0vsprintf)
    __2vsprintf                              0x00011291   Thumb Code     0  printfa.o(i.__0vsprintf)
    __c89vsprintf                            0x00011291   Thumb Code     0  printfa.o(i.__0vsprintf)
    vsprintf                                 0x00011291   Thumb Code     0  printfa.o(i.__0vsprintf)
    __ARM_clz                                0x000112b5   Thumb Code    46  depilogue.o(i.__ARM_clz)
    __ARM_common_switch8                     0x000112e3   Thumb Code    26  hal_dsi_rx_ctrl.o(i.__ARM_common_switch8)
    __scatterload_zeroinit                   0x00011391   Thumb Code    14  handlers.o(i.__scatterload_zeroinit)
    __set_errno                              0x000113a1   Thumb Code     6  errno.o(i.__set_errno)
    ap_demo                                  0x00012cdd   Thumb Code   230  ap_demo.o(i.ap_demo)
    ap_get_tp_calibration_status_01          0x00012e49   Thumb Code    28  app_tp_st_touch.o(i.ap_get_tp_calibration_status_01)
    app_ADC_IRQn_Handler                     0x000130a1   Thumb Code    22  drv_rxbr.o(i.app_ADC_IRQn_Handler)
    app_AP_NRESET_IRQn_Handler               0x000130bd   Thumb Code    32  drv_gpio.o(i.app_AP_NRESET_IRQn_Handler)
    app_EXTI_INT0_IRQn_Handler               0x000130e1   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler)
    app_EXTI_INT1_IRQn_Handler               0x000130fd   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler)
    app_EXTI_INT2_IRQn_Handler               0x00013119   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler)
    app_EXTI_INT3_IRQn_Handler               0x00013135   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler)
    app_EXTI_INT4_IRQn_Handler               0x00013151   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler)
    app_EXTI_INT5_IRQn_Handler               0x0001316d   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler)
    app_EXTI_INT6_IRQn_Handler               0x00013189   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler)
    app_EXTI_INT7_IRQn_Handler               0x000131a5   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler)
    app_HardFault_Handler                    0x000131c1   Thumb Code    12  drv_common.o(i.app_HardFault_Handler)
    app_I2C0_IRQn_Handler                    0x00013209   Thumb Code    14  drv_i2c_slave.o(i.app_I2C0_IRQn_Handler)
    app_I2C1_IRQn_Handler                    0x00013221   Thumb Code     8  drv_i2c_master.o(i.app_I2C1_IRQn_Handler)
    app_LCDC_IRQn_Handler                    0x00013231   Thumb Code   146  hal_internal_vsync.o(i.app_LCDC_IRQn_Handler)
    app_MEMC_IRQn_Handler                    0x00013361   Thumb Code   132  drv_memc.o(i.app_MEMC_IRQn_Handler)
    app_MIPI_RX_IRQn_Handler                 0x000133e9   Thumb Code   232  drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler)
    app_MIPI_TX_IRQn_Handler                 0x00013681   Thumb Code    56  drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler)
    app_PWMDET_IRQn_Handler                  0x00013721   Thumb Code    62  drv_pwm.o(i.app_PWMDET_IRQn_Handler)
    app_SPIM_IRQn_Handler                    0x00013769   Thumb Code    34  drv_spi_master.o(i.app_SPIM_IRQn_Handler)
    app_SPIS_IRQn_Handler                    0x00013799   Thumb Code   500  hal_spi_slave.o(i.app_SPIS_IRQn_Handler)
    app_SWIRE_IRQn_Handler                   0x00013999   Thumb Code    28  drv_swire.o(i.app_SWIRE_IRQn_Handler)
    app_SysTick_Handler                      0x000139b9   Thumb Code    20  drv_common.o(i.app_SysTick_Handler)
    app_TIMER0_IRQn_Handler                  0x000139d1   Thumb Code    10  drv_timer.o(i.app_TIMER0_IRQn_Handler)
    app_TIMER1_IRQn_Handler                  0x000139db   Thumb Code    10  drv_timer.o(i.app_TIMER1_IRQn_Handler)
    app_TIMER2_IRQn_Handler                  0x000139e5   Thumb Code    10  drv_timer.o(i.app_TIMER2_IRQn_Handler)
    app_TIMER3_IRQn_Handler                  0x000139ef   Thumb Code    10  drv_timer.o(i.app_TIMER3_IRQn_Handler)
    app_UART_IRQn_Handler                    0x000139f9   Thumb Code     8  drv_uart.o(i.app_UART_IRQn_Handler)
    app_VIDC_IRQn_Handler                    0x00013a01   Thumb Code    22  drv_vidc.o(i.app_VIDC_IRQn_Handler)
    app_VPRE_IRQn_Handler                    0x00013a1d   Thumb Code    22  drv_rxbr.o(i.app_VPRE_IRQn_Handler)
    app_WDG_IRQn_Handler                     0x00013a39   Thumb Code    52  drv_wdg.o(i.app_WDG_IRQn_Handler)
    app_dma_irq_handler                      0x00013a71   Thumb Code    10  drv_dma.o(i.app_dma_irq_handler)
    app_fls_ctrl_Handler                     0x00013a81   Thumb Code    38  norflash.o(i.app_fls_ctrl_Handler)
    board_Init                               0x00013ab1   Thumb Code    30  board.o(i.board_Init)
    calc_framebuffer_setting                 0x00013ad5   Thumb Code  1416  hal_internal_vsync.o(i.calc_framebuffer_setting)
    ceil                                     0x00014061   Thumb Code   180  ceil.o(i.ceil)
    dcs_packet_fifo_alloc                    0x000141d9   Thumb Code    80  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    dcs_packet_fifo_init                     0x00014231   Thumb Code    18  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    dcs_packet_free_fifo_header              0x00014249   Thumb Code    60  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    dcs_packet_get_fifo_header               0x0001428d   Thumb Code    26  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    delayMs                                  0x000142dd   Thumb Code    24  tau_delay.o(i.delayMs)
    delayUs                                  0x000142f5   Thumb Code    34  tau_delay.o(i.delayUs)
    drv_ap_rst_trig_edge_detect              0x00014319   Thumb Code    46  drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect)
    drv_chip_info_get_info                   0x00014351   Thumb Code     6  drv_chip_info.o(i.drv_chip_info_get_info)
    drv_chip_info_init                       0x0001435d   Thumb Code    56  drv_chip_info.o(i.drv_chip_info_init)
    drv_chip_rx_info_check                   0x0001439d   Thumb Code    98  drv_chip_info.o(i.drv_chip_rx_info_check)
    drv_chip_rx_init_done                    0x0001444d   Thumb Code    16  drv_chip_info.o(i.drv_chip_rx_init_done)
    drv_common_enable_systick                0x00014461   Thumb Code    70  drv_common.o(i.drv_common_enable_systick)
    drv_common_system_init                   0x000144b9   Thumb Code     8  drv_common.o(i.drv_common_system_init)
    drv_crgu_config_reset_modules            0x000144c1   Thumb Code    10  drv_crgu.o(i.drv_crgu_config_reset_modules)
    drv_crgu_set_ahb_pre_div                 0x000144d1   Thumb Code    14  drv_crgu.o(i.drv_crgu_set_ahb_pre_div)
    drv_crgu_set_ahb_src                     0x000144e5   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_ahb_src)
    drv_crgu_set_clock                       0x000144f9   Thumb Code    26  drv_crgu.o(i.drv_crgu_set_clock)
    drv_crgu_set_dpi_mux_src                 0x00014519   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dpi_mux_src)
    drv_crgu_set_dpi_pre_div                 0x0001452d   Thumb Code    18  drv_crgu.o(i.drv_crgu_set_dpi_pre_div)
    drv_crgu_set_dpi_pre_src                 0x00014545   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dpi_pre_src)
    drv_crgu_set_dsc_core_div                0x00014559   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dsc_core_div)
    drv_crgu_set_dsco_src                    0x0001456d   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dsco_src)
    drv_crgu_set_dsco_src_div                0x00014581   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dsco_src_div)
    drv_crgu_set_fb_div                      0x00014595   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_fb_div)
    drv_crgu_set_fb_src                      0x000145a9   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_fb_src)
    drv_crgu_set_lcdc_div                    0x000145bd   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_lcdc_div)
    drv_crgu_set_lcdc_src                    0x000145d1   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_lcdc_src)
    drv_crgu_set_mipi_cfg_src                0x000145e5   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_mipi_cfg_src)
    drv_crgu_set_mipi_ref_src                0x000145f9   Thumb Code    18  drv_crgu.o(i.drv_crgu_set_mipi_ref_src)
    drv_crgu_set_reset                       0x00014611   Thumb Code    20  drv_crgu.o(i.drv_crgu_set_reset)
    drv_crgu_set_rxbr_div                    0x00014629   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_rxbr_div)
    drv_crgu_set_rxbr_src                    0x0001463d   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_rxbr_src)
    drv_crgu_set_vidc_src                    0x00014651   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_vidc_src)
    drv_dma_clear_flag                       0x00014665   Thumb Code    24  drv_dma.o(i.drv_dma_clear_flag)
    drv_dma_get_channel_flag                 0x0001467d   Thumb Code    12  drv_dma.o(i.drv_dma_get_channel_flag)
    drv_dma_irq_handler                      0x00014689   Thumb Code   138  drv_dma.o(i.drv_dma_irq_handler)
    drv_dsc_dec_convert_pps_rc_parameter     0x00014719   Thumb Code    54  drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter)
    drv_dsc_dec_disable                      0x0001474f   Thumb Code    12  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    drv_dsc_dec_enable                       0x0001475d   Thumb Code    88  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    drv_dsc_dec_get_nslc                     0x000147d1   Thumb Code    10  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    drv_dsc_dec_set_u8_pps                   0x000147db   Thumb Code    40  drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps)
    drv_dsi_rx_calc_ipi_tx_delay             0x00014805   Thumb Code   244  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    drv_dsi_rx_enable_irq                    0x00014909   Thumb Code    58  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    drv_dsi_rx_get_bta_status                0x00014949   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_get_bta_status)
    drv_dsi_rx_get_compression_en            0x000149c5   Thumb Code     8  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    drv_dsi_rx_get_max_ret_size              0x000149cd   Thumb Code     6  drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size)
    drv_dsi_rx_power_up                      0x000149d3   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    drv_dsi_rx_set_ctrl_cfg                  0x000149e1   Thumb Code    32  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    drv_dsi_rx_set_ddi_cfg                   0x00014a01   Thumb Code    16  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    drv_dsi_rx_set_inten                     0x00014a11   Thumb Code     4  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    drv_dsi_rx_set_ipi_cfg                   0x00014a15   Thumb Code    16  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    drv_dsi_rx_set_lane_swap                 0x00014a25   Thumb Code    70  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    drv_dsi_rx_set_resp_cnt                  0x00014a6b   Thumb Code    38  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    drv_dsi_rx_set_up_phy                    0x00014a91   Thumb Code   256  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    drv_dsi_rx_shut_down                     0x00014b95   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    drv_dsi_tx_command_header                0x00014ba3   Thumb Code    20  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    drv_dsi_tx_command_mode_cfg              0x00014bb7   Thumb Code   108  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    drv_dsi_tx_command_put_payload           0x00014c23   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    drv_dsi_tx_config_eotp                   0x00014c27   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    drv_dsi_tx_config_int                    0x00014c3f   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    drv_dsi_tx_dpi_lpcmd_time                0x00014c47   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    drv_dsi_tx_dpi_mode                      0x00014c4f   Thumb Code    10  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    drv_dsi_tx_dpi_polarity                  0x00014c59   Thumb Code    36  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    drv_dsi_tx_edpi_cmd_size                 0x00014c7d   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    drv_dsi_tx_get_cmd_status                0x00014c81   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    drv_dsi_tx_mode                          0x00014c85   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    drv_dsi_tx_phy_clock_lane_auto_lp        0x00014c89   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    drv_dsi_tx_phy_clock_lane_req_hs         0x00014ca1   Thumb Code    26  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    drv_dsi_tx_phy_lane_mode                 0x00014cbb   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    drv_dsi_tx_phy_status_ready              0x00014cc7   Thumb Code   100  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    drv_dsi_tx_phy_status_stopstate          0x00014d2b   Thumb Code    62  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    drv_dsi_tx_phy_test_setup                0x00014d69   Thumb Code   308  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    drv_dsi_tx_phy_time_cfg                  0x00014e9d   Thumb Code    30  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    drv_dsi_tx_powerup                       0x00014ebb   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    drv_dsi_tx_response_mode                 0x00014ec3   Thumb Code    28  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    drv_dsi_tx_set_bta_ack                   0x00014edf   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    drv_dsi_tx_set_esc_div                   0x00014ef7   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    drv_dsi_tx_set_int                       0x00014f05   Thumb Code    58  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    drv_dsi_tx_set_time_out_div              0x00014f45   Thumb Code    16  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    drv_dsi_tx_set_video_chunk               0x00014f55   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    drv_dsi_tx_set_video_timing              0x00014f5d   Thumb Code    34  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    drv_dsi_tx_shutdown                      0x00014f7f   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    drv_dsi_tx_timeout_cfg                   0x00014f87   Thumb Code    38  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    drv_dsi_tx_video_mode_cfg                0x00014fad   Thumb Code   170  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    drv_dsi_tx_video_mode_disable_hact_cmd   0x00015057   Thumb Code    22  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_disable_hact_cmd)
    drv_dsi_tx_video_mode_set_lp_cmd         0x0001506d   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd)
    drv_efuse_enter_inactive                 0x00015085   Thumb Code    46  drv_efuse.o(i.drv_efuse_enter_inactive)
    drv_efuse_int_enable                     0x000150b3   Thumb Code    12  drv_efuse.o(i.drv_efuse_int_enable)
    drv_efuse_read                           0x000150bf   Thumb Code    50  drv_efuse.o(i.drv_efuse_read)
    drv_efuse_read_req                       0x000150f1   Thumb Code    24  drv_efuse.o(i.drv_efuse_read_req)
    drv_gpio_set_ioe                         0x00015109   Thumb Code    26  drv_gpio.o(i.drv_gpio_set_ioe)
    drv_gpio_set_mode0                       0x00015129   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode0)
    drv_gpio_set_mode1                       0x00015139   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode1)
    drv_gpio_set_mode2                       0x00015149   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode2)
    drv_gpio_set_mode3                       0x00015159   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode3)
    drv_lcdc_config_bypass                   0x00015189   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_config_bypass)
    drv_lcdc_config_ccm                      0x000151a1   Thumb Code    48  drv_lcdc.o(i.drv_lcdc_config_ccm)
    drv_lcdc_config_disp_mode                0x000151d1   Thumb Code    22  drv_lcdc.o(i.drv_lcdc_config_disp_mode)
    drv_lcdc_config_dpi_polarity             0x000151e7   Thumb Code    36  drv_lcdc.o(i.drv_lcdc_config_dpi_polarity)
    drv_lcdc_config_dpi_timing               0x0001520b   Thumb Code    38  drv_lcdc.o(i.drv_lcdc_config_dpi_timing)
    drv_lcdc_config_edpi_mode                0x00015231   Thumb Code    22  drv_lcdc.o(i.drv_lcdc_config_edpi_mode)
    drv_lcdc_config_endianness               0x00015247   Thumb Code    22  drv_lcdc.o(i.drv_lcdc_config_endianness)
    drv_lcdc_config_input_size               0x0001525d   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_config_input_size)
    drv_lcdc_config_int                      0x00015269   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_config_int)
    drv_lcdc_config_int_single               0x00015287   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_int_single)
    drv_lcdc_config_overwrite                0x000152a9   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_overwrite)
    drv_lcdc_config_overwrite_rgb            0x000152cb   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    drv_lcdc_config_partial_display_area     0x000152d7   Thumb Code    26  drv_lcdc.o(i.drv_lcdc_config_partial_display_area)
    drv_lcdc_config_partial_display_enable   0x000152f1   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_partial_display_enable)
    drv_lcdc_config_scale_up_coef            0x00015313   Thumb Code    26  drv_lcdc.o(i.drv_lcdc_config_scale_up_coef)
    drv_lcdc_config_scale_up_step            0x0001532d   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_config_scale_up_step)
    drv_lcdc_config_src_parameter            0x00015339   Thumb Code    76  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    drv_lcdc_config_thresh                   0x00015385   Thumb Code     6  drv_lcdc.o(i.drv_lcdc_config_thresh)
    drv_lcdc_ctrl_flow                       0x0001538b   Thumb Code    18  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    drv_lcdc_enable_shadow_reg               0x0001539d   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    drv_lcdc_set_int                         0x000153bd   Thumb Code    58  drv_lcdc.o(i.drv_lcdc_set_int)
    drv_lcdc_set_prefetch                    0x000153fd   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_set_prefetch)
    drv_lcdc_set_video_hw_mode               0x00015415   Thumb Code    20  drv_lcdc.o(i.drv_lcdc_set_video_hw_mode)
    drv_lcdc_start                           0x00015429   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_start)
    drv_memc_clear_status                    0x00015449   Thumb Code    12  drv_memc.o(i.drv_memc_clear_status)
    drv_memc_enable_irq                      0x00015455   Thumb Code    58  drv_memc.o(i.drv_memc_enable_irq)
    drv_memc_gen_a_tear_signal               0x00015495   Thumb Code    12  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    drv_memc_get_status                      0x000154a1   Thumb Code    18  drv_memc.o(i.drv_memc_get_status)
    drv_memc_rate_transfer_sel               0x000154b3   Thumb Code    16  drv_memc.o(i.drv_memc_rate_transfer_sel)
    drv_memc_sel_vsync                       0x000154c3   Thumb Code    14  drv_memc.o(i.drv_memc_sel_vsync)
    drv_memc_set_active_height               0x000154d1   Thumb Code    14  drv_memc.o(i.drv_memc_set_active_height)
    drv_memc_set_data_mode                   0x000154e5   Thumb Code    12  drv_memc.o(i.drv_memc_set_data_mode)
    drv_memc_set_double_buffer               0x000154f1   Thumb Code    16  drv_memc.o(i.drv_memc_set_double_buffer)
    drv_memc_set_double_buffer_reverse       0x00015501   Thumb Code    18  drv_memc.o(i.drv_memc_set_double_buffer_reverse)
    drv_memc_set_fs_en_conditions            0x00015513   Thumb Code    16  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    drv_memc_set_inten                       0x00015523   Thumb Code    20  drv_memc.o(i.drv_memc_set_inten)
    drv_memc_set_lcdc_st_conditions          0x00015539   Thumb Code    18  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    drv_memc_set_ltpo_mode                   0x00015551   Thumb Code    26  drv_memc.o(i.drv_memc_set_ltpo_mode)
    drv_memc_set_tear_mode                   0x0001556b   Thumb Code    14  drv_memc.o(i.drv_memc_set_tear_mode)
    drv_memc_set_tear_waveform               0x00015579   Thumb Code    34  drv_memc.o(i.drv_memc_set_tear_waveform)
    drv_memc_set_vidc_sync_cnt               0x000155a1   Thumb Code    14  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    drv_param_init_get_ccm                   0x000155b1   Thumb Code     4  drv_param_init.o(i.drv_param_init_get_ccm)
    drv_param_init_get_scld_filter_h         0x000155b9   Thumb Code    12  drv_param_init.o(i.drv_param_init_get_scld_filter_h)
    drv_param_init_get_scld_filter_v         0x000155cd   Thumb Code    12  drv_param_init.o(i.drv_param_init_get_scld_filter_v)
    drv_param_init_get_sclu_filter           0x000155e1   Thumb Code     4  drv_param_init.o(i.drv_param_init_get_sclu_filter)
    drv_param_init_set_ccm                   0x000155e9   Thumb Code    14  drv_param_init.o(i.drv_param_init_set_ccm)
    drv_param_init_set_scld_filter           0x000155fd   Thumb Code    92  drv_param_init.o(i.drv_param_init_set_scld_filter)
    drv_param_p2r_filter_init                0x00015661   Thumb Code    30  drv_param_init.o(i.drv_param_p2r_filter_init)
    drv_phy_enable_calibration               0x00015685   Thumb Code    12  drv_phy_common.o(i.drv_phy_enable_calibration)
    drv_phy_get_calibration                  0x00015695   Thumb Code    50  drv_phy_common.o(i.drv_phy_get_calibration)
    drv_phy_get_pll_para                     0x000156d1   Thumb Code    88  drv_phy_common.o(i.drv_phy_get_pll_para)
    drv_phy_get_rate_para                    0x00015731   Thumb Code    76  drv_phy_common.o(i.drv_phy_get_rate_para)
    drv_phy_test_clear                       0x00015785   Thumb Code    16  drv_phy_common.o(i.drv_phy_test_clear)
    drv_phy_test_lock                        0x00015795   Thumb Code    24  drv_phy_common.o(i.drv_phy_test_lock)
    drv_phy_test_write_1_byte                0x000157ad   Thumb Code    32  drv_phy_common.o(i.drv_phy_test_write_1_byte)
    drv_phy_test_write_2_byte                0x000157cd   Thumb Code    38  drv_phy_common.o(i.drv_phy_test_write_2_byte)
    drv_phy_test_write_code                  0x000157f3   Thumb Code    30  drv_phy_common.o(i.drv_phy_test_write_code)
    drv_pwr_set_pvd_mode                     0x00015831   Thumb Code    18  drv_pwr.o(i.drv_pwr_set_pvd_mode)
    drv_pwr_set_system_clk_src               0x00015849   Thumb Code    44  drv_pwr.o(i.drv_pwr_set_system_clk_src)
    drv_rxbr_clear_pkt_buffer                0x000158c7   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    drv_rxbr_clear_status0                   0x000158d1   Thumb Code     4  drv_rxbr.o(i.drv_rxbr_clear_status0)
    drv_rxbr_enable_irq                      0x000158d5   Thumb Code    90  drv_rxbr.o(i.drv_rxbr_enable_irq)
    drv_rxbr_frame_drop_cfg                  0x00015931   Thumb Code    16  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    drv_rxbr_get_clk                         0x00015945   Thumb Code    66  drv_rxbr.o(i.drv_rxbr_get_clk)
    drv_rxbr_get_col_addr                    0x000159a9   Thumb Code     4  drv_rxbr.o(i.drv_rxbr_get_col_addr)
    drv_rxbr_get_page_addr                   0x000159bf   Thumb Code     4  drv_rxbr.o(i.drv_rxbr_get_page_addr)
    drv_rxbr_get_pkt_buf_error_status        0x000159c3   Thumb Code    12  drv_rxbr.o(i.drv_rxbr_get_pkt_buf_error_status)
    drv_rxbr_hline_rcv0_cfg                  0x000159f7   Thumb Code    12  drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg)
    drv_rxbr_hline_rcv1_cfg                  0x00015a03   Thumb Code    12  drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg)
    drv_rxbr_hline_rcv_cfg                   0x00015a0f   Thumb Code     8  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    drv_rxbr_register_irq0_callback          0x00015a19   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_register_irq0_callback)
    drv_rxbr_register_irq1_callback          0x00015a25   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    drv_rxbr_set_ack_pkt_header              0x00015a31   Thumb Code    20  drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header)
    drv_rxbr_set_color_format                0x00015a45   Thumb Code    20  drv_rxbr.o(i.drv_rxbr_set_color_format)
    drv_rxbr_set_filter_regs                 0x00015a59   Thumb Code    18  drv_rxbr.o(i.drv_rxbr_set_filter_regs)
    drv_rxbr_set_inten                       0x00015a6b   Thumb Code    20  drv_rxbr.o(i.drv_rxbr_set_inten)
    drv_rxbr_set_ltpo_drop_th                0x00015a7f   Thumb Code    16  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    drv_rxbr_set_usr_cfg                     0x00015a8f   Thumb Code    38  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    drv_rxbr_set_usr_col                     0x00015ab5   Thumb Code     8  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    drv_rxbr_set_usr_row                     0x00015abd   Thumb Code     8  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    drv_swire_set_int                        0x00015ac5   Thumb Code    76  drv_swire.o(i.drv_swire_set_int)
    drv_sys_cfg_clear_all_int                0x00015b19   Thumb Code     8  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    drv_sys_cfg_clear_pending                0x00015b25   Thumb Code    32  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    drv_sys_cfg_sel_ap_rst_lvl_trig          0x00015b4d   Thumb Code    18  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig)
    drv_sys_cfg_set_int                      0x00015b65   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    drv_timer_enable                         0x00015ba3   Thumb Code    32  drv_timer.o(i.drv_timer_enable)
    drv_timer_get_instance                   0x00015bc5   Thumb Code    10  drv_timer.o(i.drv_timer_get_instance)
    drv_timer_set_compare_val                0x00015c19   Thumb Code    16  drv_timer.o(i.drv_timer_set_compare_val)
    drv_timer_set_int                        0x00015c29   Thumb Code    80  drv_timer.o(i.drv_timer_set_int)
    drv_tx_phy_test_enter                    0x00015c87   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    drv_tx_phy_test_exit                     0x00015ca3   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    drv_vidc_clear_irq                       0x00015cf5   Thumb Code     8  drv_vidc.o(i.drv_vidc_clear_irq)
    drv_vidc_enable                          0x00015cfd   Thumb Code    24  drv_vidc.o(i.drv_vidc_enable)
    drv_vidc_enable_irq                      0x00015d15   Thumb Code    58  drv_vidc.o(i.drv_vidc_enable_irq)
    drv_vidc_get_irq_status                  0x00015d55   Thumb Code    18  drv_vidc.o(i.drv_vidc_get_irq_status)
    drv_vidc_init_module_enable              0x00015d69   Thumb Code    36  drv_vidc.o(i.drv_vidc_init_module_enable)
    drv_vidc_register_callback               0x00015d91   Thumb Code     6  drv_vidc.o(i.drv_vidc_register_callback)
    drv_vidc_reset                           0x00015d9d   Thumb Code     6  drv_vidc.o(i.drv_vidc_reset)
    drv_vidc_set_dst_parameter               0x00015da3   Thumb Code    60  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    drv_vidc_set_irqen                       0x00015ddf   Thumb Code    20  drv_vidc.o(i.drv_vidc_set_irqen)
    drv_vidc_set_mirror                      0x00015df3   Thumb Code    16  drv_vidc.o(i.drv_vidc_set_mirror)
    drv_vidc_set_p2r_hcoef0                  0x00015e03   Thumb Code     8  drv_vidc.o(i.drv_vidc_set_p2r_hcoef0)
    drv_vidc_set_p2r_hinitb                  0x00015e0b   Thumb Code    38  drv_vidc.o(i.drv_vidc_set_p2r_hinitb)
    drv_vidc_set_p2r_hinitr                  0x00015e31   Thumb Code    38  drv_vidc.o(i.drv_vidc_set_p2r_hinitr)
    drv_vidc_set_pentile_swap                0x00015e59   Thumb Code    18  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    drv_vidc_set_pu_ctrl                     0x00015e71   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    drv_vidc_set_rotation                    0x00015e7b   Thumb Code    16  drv_vidc.o(i.drv_vidc_set_rotation)
    drv_vidc_set_scld_hcoef0                 0x00015e8b   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    drv_vidc_set_scld_hcoef1                 0x00015e95   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    drv_vidc_set_scld_step                   0x00015e9f   Thumb Code    18  drv_vidc.o(i.drv_vidc_set_scld_step)
    drv_vidc_set_scld_vcoef0                 0x00015eb1   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    drv_vidc_set_scld_vcoef1                 0x00015ebb   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    drv_vidc_set_src_parameter               0x00015ec5   Thumb Code    22  drv_vidc.o(i.drv_vidc_set_src_parameter)
    drv_wdg_clear_counter                    0x00015edd   Thumb Code    12  drv_wdg.o(i.drv_wdg_clear_counter)
    drv_wdg_set_int                          0x00015f0d   Thumb Code    60  drv_wdg.o(i.drv_wdg_set_int)
    fls_clr_interrupt_flag                   0x00015f4d   Thumb Code    10  drv_fls.o(i.fls_clr_interrupt_flag)
    fputc                                    0x00015f57   Thumb Code    20  tau_log.o(i.fputc)
    hal_dsi_rx_ctrl_create_handle            0x00015fbd   Thumb Code    48  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    hal_dsi_rx_ctrl_dsc_async_handler        0x00015ff1   Thumb Code    34  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler)
    hal_dsi_rx_ctrl_gen_a_tear_signal        0x00016019   Thumb Code    32  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal)
    hal_dsi_rx_ctrl_get_max_ret_size         0x00016041   Thumb Code    30  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size)
    hal_dsi_rx_ctrl_init                     0x00016069   Thumb Code   144  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    hal_dsi_rx_ctrl_pre_init_pps             0x00016859   Thumb Code    56  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    hal_dsi_rx_ctrl_restart                  0x00016895   Thumb Code    72  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart)
    hal_dsi_rx_ctrl_send_ack_cmd             0x000168e5   Thumb Code   212  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd)
    hal_dsi_rx_ctrl_set_cus_esc_clk          0x000169d5   Thumb Code    34  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk)
    hal_dsi_rx_ctrl_set_cus_scld_filter      0x00016a01   Thumb Code    98  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter)
    hal_dsi_rx_ctrl_set_cus_sync_line        0x00016a6d   Thumb Code    44  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line)
    hal_dsi_rx_ctrl_set_tear_mode_ex         0x00016b4b   Thumb Code    14  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex)
    hal_dsi_rx_ctrl_start                    0x00016b59   Thumb Code    46  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    hal_dsi_rx_ctrl_toggle_resolution        0x00016b95   Thumb Code    28  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    hal_dsi_tx_ctrl_create_handle            0x000171a1   Thumb Code    34  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    hal_dsi_tx_ctrl_enter_init_panel_mode    0x000171cd   Thumb Code    68  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode)
    hal_dsi_tx_ctrl_exit_init_panel_mode     0x00017219   Thumb Code    32  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode)
    hal_dsi_tx_ctrl_init                     0x00017241   Thumb Code   154  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    hal_dsi_tx_ctrl_panel_reset_pin          0x00017309   Thumb Code    12  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin)
    hal_dsi_tx_ctrl_set_ccm                  0x00017315   Thumb Code    28  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm)
    hal_dsi_tx_ctrl_set_overwrite_rgb        0x00017335   Thumb Code    16  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    hal_dsi_tx_ctrl_set_partial_disp         0x00017349   Thumb Code    12  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp)
    hal_dsi_tx_ctrl_set_partial_disp_area    0x00017359   Thumb Code    30  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area)
    hal_dsi_tx_ctrl_start                    0x0001737d   Thumb Code   150  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    hal_dsi_tx_ctrl_write_array_cmd          0x00017425   Thumb Code   236  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd)
    hal_dsi_tx_ctrl_write_cmd                0x00017515   Thumb Code   200  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    hal_gpio_init_output                     0x000177c5   Thumb Code    34  hal_gpio.o(i.hal_gpio_init_output)
    hal_gpio_set_mode                        0x000177ed   Thumb Code    90  hal_gpio.o(i.hal_gpio_set_mode)
    hal_gpio_set_output_data                 0x0001784d   Thumb Code     8  hal_gpio.o(i.hal_gpio_set_output_data)
    hal_internal_check_video_auto_sync       0x00017855   Thumb Code    18  hal_internal_vsync.o(i.hal_internal_check_video_auto_sync)
    hal_internal_init_memc                   0x0001786d   Thumb Code   170  hal_internal_vsync.o(i.hal_internal_init_memc)
    hal_internal_rx_dcs_async_handler        0x00017969   Thumb Code    42  hal_internal_vsync.o(i.hal_internal_rx_dcs_async_handler)
    hal_internal_rx_dcs_polling              0x00017995   Thumb Code    78  hal_internal_vsync.o(i.hal_internal_rx_dcs_polling)
    hal_internal_sync_get_fb_setting         0x000179ed   Thumb Code    12  hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting)
    hal_internal_sync_get_hight_performan_mode 0x000179fd   Thumb Code    10  hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode)
    hal_internal_sync_input_resolution_change 0x00017a0d   Thumb Code   438  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    hal_internal_vsync_deinit                0x00017c39   Thumb Code    30  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    hal_internal_vsync_get_sync_line         0x00017c61   Thumb Code    18  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    hal_internal_vsync_get_tear_mode         0x00017c79   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_tear_mode)
    hal_internal_vsync_get_tx_state          0x00017c85   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    hal_internal_vsync_init_rx               0x00017c91   Thumb Code   274  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    hal_internal_vsync_init_tx               0x00017dd1   Thumb Code   172  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    hal_internal_vsync_set_auto_hw_filter    0x00017e81   Thumb Code   132  hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter)
    hal_internal_vsync_set_rx_state          0x00017f11   Thumb Code    30  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    hal_internal_vsync_set_sync_line         0x00017f35   Thumb Code    64  hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line)
    hal_internal_vsync_set_tear_mode         0x00017f79   Thumb Code    72  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    hal_internal_vsync_set_tx_state          0x00017fc9   Thumb Code   122  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    hal_intl_svs_deinit_tx                   0x0001804d   Thumb Code    10  hal_internal_soft_sync.o(i.hal_intl_svs_deinit_tx)
    hal_intl_svs_handle                      0x0001805d   Thumb Code    24  hal_internal_soft_sync.o(i.hal_intl_svs_handle)
    hal_intl_svs_init_rx                     0x00018081   Thumb Code   108  hal_internal_soft_sync.o(i.hal_intl_svs_init_rx)
    hal_intl_svs_init_tx                     0x000180f9   Thumb Code    16  hal_internal_soft_sync.o(i.hal_intl_svs_init_tx)
    hal_intl_svs_set_sync_coef               0x0001810d   Thumb Code     8  hal_internal_soft_sync.o(i.hal_intl_svs_set_sync_coef)
    hal_intl_svs_update_rxbr_clk             0x00018119   Thumb Code    52  hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk)
    hal_system_enable_systick                0x000185c1   Thumb Code     8  hal_system.o(i.hal_system_enable_systick)
    hal_system_init                          0x000185c9   Thumb Code   104  hal_system.o(i.hal_system_init)
    hal_system_init_console                  0x00018651   Thumb Code    28  hal_system.o(i.hal_system_init_console)
    hal_system_set_phy_calibration           0x0001866d   Thumb Code     8  hal_system.o(i.hal_system_set_phy_calibration)
    hal_uart_init                            0x000186a5   Thumb Code   126  hal_uart.o(i.hal_uart_init)
    hal_uart_transmit_blocking               0x00018731   Thumb Code    12  hal_uart.o(i.hal_uart_transmit_blocking)
    handle_init                              0x00018741   Thumb Code   140  irq_redirect .o(i.handle_init)
    main                                     0x0001895d   Thumb Code    10  main.o(i.main)
    sqrt                                     0x000196d9   Thumb Code    66  sqrt.o(i.sqrt)
    panel_init_code                          0x00019e7c   Data        7814  ap_demo.o(.constdata)
    Region$$Table$$Base                      0x0001c1ec   Number         0  anon$$obj.o(Region$$Table)
    Region$$Table$$Limit                     0x0001c21c   Number         0  anon$$obj.o(Region$$Table)
    g_fun_handle                             0x00070100   Data         192  irq_redirect .o(.ARM.__AT_0x00070100)
    s_power_up_flag                          0x000701d7   Data           1  ap_demo.o(.data)
    panel_mode                               0x000701d8   Data           1  ap_demo.o(.data)
    s_tp_delay_count                         0x000701e4   Data           2  ap_demo.o(.data)
    panel_r                                  0x000701e6   Data           2  ap_demo.o(.data)
    panel_g                                  0x000701e8   Data           2  ap_demo.o(.data)
    panel_b                                  0x000701ea   Data           2  ap_demo.o(.data)
    s_heartbeat                              0x000701f8   Data           4  ap_demo.o(.data)
    rx_filter_1080_h_4_96                    0x00070200   Data         256  ap_demo.o(.data)
    rx_filter_2400_v_4_96                    0x00070300   Data         256  ap_demo.o(.data)
    g_tp_sleep_delay_count                   0x00070400   Data           1  app_tp_st_touch.o(.data)
    g_tp_wakeup_response                     0x00070401   Data           1  app_tp_st_touch.o(.data)
    s_tp_wakeup                              0x00070402   Data           1  app_tp_st_touch.o(.data)
    st_touch_init_sensor_off                 0x00070405   Data           3  app_tp_st_touch.o(.data)
    st_touch_init_sensor_on                  0x00070408   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_reset                 0x0007040b   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_FpnlInit              0x0007040e   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_PnlInit               0x00070411   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_SvCfg                 0x00070414   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_SvCx                  0x00070417   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_SvPnl                 0x0007041a   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_clearfifo             0x0007041d   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_clkreset              0x00070420   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_TuneM                 0x00070423   Data           4  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_TuneS                 0x00070427   Data           4  app_tp_st_touch.o(.data)
    phone_reg_coord_back_X61                 0x0007042b   Data          16  app_tp_st_touch.o(.data)
    phone_data_E4                            0x0007043c   Data           1  app_tp_for_custom_s8.o(.data)
    tp_flag                                  0x0007043d   Data           1  app_tp_for_custom_s8.o(.data)
    g_phone_output_int_pad                   0x0007043e   Data           1  app_tp_for_custom_s8.o(.data)
    tp_sleep_in                              0x0007043f   Data           1  app_tp_for_custom_s8.o(.data)
    tp_sleep_count                           0x00070440   Data           1  app_tp_for_custom_s8.o(.data)
    sleep_double_EN                          0x00070441   Data           1  app_tp_for_custom_s8.o(.data)
    Flag_EA_EN                               0x00070442   Data           1  app_tp_for_custom_s8.o(.data)
    Flag_touch_count                         0x00070443   Data           1  app_tp_for_custom_s8.o(.data)
    touchnum_bak                             0x00070444   Data           1  app_tp_for_custom_s8.o(.data)
    Flag_blacklight_EN                       0x00070445   Data           1  app_tp_for_custom_s8.o(.data)
    phone_data_B1                            0x0007044e   Data           2  app_tp_for_custom_s8.o(.data)
    phone_reg_coord_back                     0x00070458   Data         200  app_tp_for_custom_s8.o(.data)
    g_sof_gen_te_func                        0x00070534   Data           4  hal_internal_vsync.o(.data)
    g_systick_cb_func                        0x00070548   Data           4  drv_common.o(.data)
    g_system_clock                           0x0007054c   Data           4  drv_common.o(.data)
    g_scld_fhd_filter_h                      0x0007055c   Data         256  drv_param_init.o(.data)
    g_scld_fhd_filter_v                      0x0007065c   Data         256  drv_param_init.o(.data)
    g_scld_hd_filter_h                       0x0007075c   Data         256  drv_param_init.o(.data)
    g_scld_hd_filter_v                       0x0007085c   Data         256  drv_param_init.o(.data)
    g_sclu_lanczos_filter                    0x0007095c   Data         128  drv_param_init.o(.data)
    g_ccm_setting                            0x000709dc   Data          36  drv_param_init.o(.data)
    g_int_rxbr_irq0_cb_func                  0x00070a08   Data           4  drv_rxbr.o(.data)
    g_int_rxbr_irq1_cb_func                  0x00070a0c   Data           4  drv_rxbr.o(.data)
    g_int_vidc_cb_func                       0x00070a10   Data           4  drv_vidc.o(.data)
    g_fls_w_cmd                              0x00070a24   Data           1  norflash.o(.data)
    g_fls_r_cmd                              0x00070a25   Data           1  norflash.o(.data)
    g_fls_write_en_status                    0x00070a26   Data           1  norflash.o(.data)
    isFlsTransferEnd                         0x00070a27   Data           1  norflash.o(.data)
    isFlsFifoReq                             0x00070a28   Data           1  norflash.o(.data)
    isNandWriteCompleted                     0x00070a29   Data           1  norflash.o(.data)
    isNandReadCompleted                      0x00070a2a   Data           1  norflash.o(.data)
    g_fls_error_info                         0x00070a30   Data           6  norflash.o(.data)
    __stdout                                 0x00070ab0   Data           4  stdout.o(.data)
    string                                   0x00070bec   Data         256  tau_log.o(.bss)
    hal_dmahandle                            0x00070cec   Data         160  hal_uart.o(.bss)
    hal_uarthandle_dma                       0x00070d8c   Data          32  hal_uart.o(.bss)
    hal_uart_handle_global                   0x00070dac   Data          16  hal_uart.o(.bss)
    g_vsync_hande                            0x00070dbc   Data          84  hal_internal_vsync.o(.bss)
    g_dcs_execute_table                      0x00070e10   Data        2048  hal_internal_vsync.o(.bss)
    g_spis_ctrl_handle                       0x000717cc   Data          32  hal_spi_slave.o(.bss)
    g_packet_fifo                            0x000717ec   Data        4144  dcs_packet_fifo.o(.bss)
    __stack_limit                            0x00072820   Data           0  startup_armcm0.o(STACK)
    __initial_sp                             0x00073820   Data           0  startup_armcm0.o(STACK)



==============================================================================

Memory Map of the image

  Image Entry point : 0x000100c1

  Load Region LR_IROM2 (Base: 0x00010000, Size: 0x0000cb04, Max: 0x00010000, ABSOLUTE, COMPRESSED[0x0000c748])

    Execution Region ER_IROM2 (Exec base: 0x00010000, Load base: 0x00010000, Size: 0x0000c21c, Max: 0x00010000, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00010000   0x00010000   0x000000c0   Data   RO          562    RESET               startup_armcm0.o
    0x000100c0   0x000100c0   0x00000000   Code   RO         2740  * .ARM.Collect$$$$00000000  mc_p.l(entry.o)
    0x000100c0   0x000100c0   0x00000004   Code   RO         3052    .ARM.Collect$$$$00000001  mc_p.l(entry2.o)
    0x000100c4   0x000100c4   0x00000004   Code   RO         3055    .ARM.Collect$$$$00000004  mc_p.l(entry5.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         3057    .ARM.Collect$$$$00000008  mc_p.l(entry7b.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         3059    .ARM.Collect$$$$0000000A  mc_p.l(entry8b.o)
    0x000100c8   0x000100c8   0x00000008   Code   RO         3060    .ARM.Collect$$$$0000000B  mc_p.l(entry9a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         3062    .ARM.Collect$$$$0000000D  mc_p.l(entry10a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         3064    .ARM.Collect$$$$0000000F  mc_p.l(entry11a.o)
    0x000100d0   0x000100d0   0x00000004   Code   RO         3053    .ARM.Collect$$$$00002712  mc_p.l(entry2.o)
    0x000100d4   0x000100d4   0x00000078   Code   RO          563    .text               startup_armcm0.o
    0x0001014c   0x0001014c   0x0000002c   Code   RO         2743    .text               mc_p.l(uidiv.o)
    0x00010178   0x00010178   0x00000028   Code   RO         2745    .text               mc_p.l(idiv.o)
    0x000101a0   0x000101a0   0x00000024   Code   RO         2747    .text               mc_p.l(memcpya.o)
    0x000101c4   0x000101c4   0x00000024   Code   RO         2749    .text               mc_p.l(memseta.o)
    0x000101e8   0x000101e8   0x000000b2   Code   RO         3014    .text               mf_p.l(fadd.o)
    0x0001029a   0x0001029a   0x0000007a   Code   RO         3016    .text               mf_p.l(fmul.o)
    0x00010314   0x00010314   0x0000007c   Code   RO         3018    .text               mf_p.l(fdiv.o)
    0x00010390   0x00010390   0x00000018   Code   RO         3020    .text               mf_p.l(fscalb.o)
    0x000103a8   0x000103a8   0x00000164   Code   RO         3022    .text               mf_p.l(dadd.o)
    0x0001050c   0x0001050c   0x000000d0   Code   RO         3024    .text               mf_p.l(dmul.o)
    0x000105dc   0x000105dc   0x000000f0   Code   RO         3026    .text               mf_p.l(ddiv.o)
    0x000106cc   0x000106cc   0x00000016   Code   RO         3028    .text               mf_p.l(fflti.o)
    0x000106e2   0x000106e2   0x0000000e   Code   RO         3030    .text               mf_p.l(ffltui.o)
    0x000106f0   0x000106f0   0x0000001c   Code   RO         3034    .text               mf_p.l(dfltui.o)
    0x0001070c   0x0001070c   0x00000032   Code   RO         3036    .text               mf_p.l(ffixi.o)
    0x0001073e   0x0001073e   0x00000028   Code   RO         3038    .text               mf_p.l(ffixui.o)
    0x00010766   0x00010766   0x00000002   PAD
    0x00010768   0x00010768   0x00000048   Code   RO         3040    .text               mf_p.l(dfixi.o)
    0x000107b0   0x000107b0   0x0000003c   Code   RO         3042    .text               mf_p.l(dfixui.o)
    0x000107ec   0x000107ec   0x00000028   Code   RO         3044    .text               mf_p.l(f2d.o)
    0x00010814   0x00010814   0x00000028   Code   RO         3046    .text               mf_p.l(cdcmple.o)
    0x0001083c   0x0001083c   0x00000014   Code   RO         3048    .text               mf_p.l(cfcmple.o)
    0x00010850   0x00010850   0x00000014   Code   RO         3050    .text               mf_p.l(cfrcmple.o)
    0x00010864   0x00010864   0x00000060   Code   RO         3067    .text               mc_p.l(uldiv.o)
    0x000108c4   0x000108c4   0x00000020   Code   RO         3069    .text               mc_p.l(llshl.o)
    0x000108e4   0x000108e4   0x00000022   Code   RO         3071    .text               mc_p.l(llushr.o)
    0x00010906   0x00010906   0x00000026   Code   RO         3073    .text               mc_p.l(llsshr.o)
    0x0001092c   0x0001092c   0x00000000   Code   RO         3082    .text               mc_p.l(iusefp.o)
    0x0001092c   0x0001092c   0x00000082   Code   RO         3083    .text               mf_p.l(fepilogue.o)
    0x000109ae   0x000109ae   0x000000be   Code   RO         3085    .text               mf_p.l(depilogue.o)
    0x00010a6c   0x00010a6c   0x000000a2   Code   RO         3089    .text               mf_p.l(dsqrt.o)
    0x00010b0e   0x00010b0e   0x00000002   PAD
    0x00010b10   0x00010b10   0x00000040   Code   RO         3091    .text               mf_p.l(dfixul.o)
    0x00010b50   0x00010b50   0x00000028   Code   RO         3093    .text               mf_p.l(cdrcmple.o)
    0x00010b78   0x00010b78   0x00000024   Code   RO         3095    .text               mc_p.l(init.o)
    0x00010b9c   0x00010b9c   0x00000056   Code   RO         3105    .text               mc_p.l(__dczerorl2.o)
    0x00010bf2   0x00010bf2   0x00000002   PAD
    0x00010bf4   0x00010bf4   0x00000018   Code   RO         2184    i.ADC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c0c   0x00010c0c   0x00000018   Code   RO         2185    i.AP_NRESET_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c24   0x00010c24   0x00000014   Code   RO         2186    i.DMA_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c38   0x00010c38   0x0000001c   Code   RO         2187    i.EXTI_INT0_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c54   0x00010c54   0x0000001c   Code   RO         2188    i.EXTI_INT1_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c70   0x00010c70   0x0000001c   Code   RO         2189    i.EXTI_INT2_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c8c   0x00010c8c   0x0000001c   Code   RO         2190    i.EXTI_INT3_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010ca8   0x00010ca8   0x0000001c   Code   RO         2191    i.EXTI_INT4_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010cc4   0x00010cc4   0x0000001c   Code   RO         2192    i.EXTI_INT5_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010ce0   0x00010ce0   0x0000001c   Code   RO         2193    i.EXTI_INT6_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010cfc   0x00010cfc   0x0000001c   Code   RO         2194    i.EXTI_INT7_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010d18   0x00010d18   0x00000014   Code   RO         2195    i.FLSCTRL_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010d2c   0x00010d2c   0x0000004e   Code   RO          103    i.Gpio_swire_output  ap_demo.o
    0x00010d7a   0x00010d7a   0x00000002   PAD
    0x00010d7c   0x00010d7c   0x00000014   Code   RO         2196    i.HardFault_Handler  CVWL568.lib(irq_redirect .o)
    0x00010d90   0x00010d90   0x00000018   Code   RO         2197    i.I2C0_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010da8   0x00010da8   0x00000018   Code   RO         2198    i.I2C1_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010dc0   0x00010dc0   0x00000018   Code   RO         2199    i.LCDC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010dd8   0x00010dd8   0x00000028   Code   RO         1069    i.LOG_printf        CVWL568.lib(tau_log.o)
    0x00010e00   0x00010e00   0x00000018   Code   RO         2200    i.MEMC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e18   0x00010e18   0x00000018   Code   RO         2201    i.MIPI_RX_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e30   0x00010e30   0x00000018   Code   RO         2202    i.MIPI_TX_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e48   0x00010e48   0x0000001c   Code   RO         2203    i.PWMDET_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e64   0x00010e64   0x0000001c   Code   RO         2204    i.SPIM_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e80   0x00010e80   0x0000001c   Code   RO         2205    i.SPIS_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e9c   0x00010e9c   0x0000001c   Code   RO         2206    i.SWIRE_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010eb8   0x00010eb8   0x00000018   Code   RO         2207    i.SysTick_Handler   CVWL568.lib(irq_redirect .o)
    0x00010ed0   0x00010ed0   0x00000018   Code   RO         2208    i.TIMER0_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010ee8   0x00010ee8   0x00000018   Code   RO         2209    i.TIMER1_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010f00   0x00010f00   0x00000018   Code   RO         2210    i.TIMER2_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010f18   0x00010f18   0x00000018   Code   RO         2211    i.TIMER3_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010f30   0x00010f30   0x0000001c   Code   RO         2607    i.UART0_IRQ_Handle  CVWL568.lib(drv_uart.o)
    0x00010f4c   0x00010f4c   0x00000002   Code   RO         2611    i.UART_DisableDma   CVWL568.lib(drv_uart.o)
    0x00010f4e   0x00010f4e   0x00000004   Code   RO         2617    i.UART_GetInstance  CVWL568.lib(drv_uart.o)
    0x00010f52   0x00010f52   0x00000002   PAD
    0x00010f54   0x00010f54   0x00000018   Code   RO         2212    i.UART_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010f6c   0x00010f6c   0x00000024   Code   RO         2625    i.UART_ResetRxFIFO  CVWL568.lib(drv_uart.o)
    0x00010f90   0x00010f90   0x00000048   Code   RO         2628    i.UART_SetBaudRate  CVWL568.lib(drv_uart.o)
    0x00010fd8   0x00010fd8   0x0000001a   Code   RO         2629    i.UART_SwitchSCLK   CVWL568.lib(drv_uart.o)
    0x00010ff2   0x00010ff2   0x0000000e   Code   RO         3099    i.__scatterload_copy  mc_p.l(handlers.o)
    0x00011000   0x00011000   0x00000014   Data   RO         1206    .ARM.__at_0x11000   CVWL568.lib(drv_common.o)
    0x00011014   0x00011014   0x00000002   Code   RO         3100    i.__scatterload_null  mc_p.l(handlers.o)
    0x00011016   0x00011016   0x00000002   PAD
    0x00011018   0x00011018   0x00000004   Data   RO         1207    .ARM.__at_0x11018   CVWL568.lib(drv_common.o)
    0x0001101c   0x0001101c   0x00000134   Code   RO         2631    i.UART_TransferHandleIRQ  CVWL568.lib(drv_uart.o)
    0x00011150   0x00011150   0x0000001a   Code   RO         2633    i.UART_WriteBlocking  CVWL568.lib(drv_uart.o)
    0x0001116a   0x0001116a   0x00000002   PAD
    0x0001116c   0x0001116c   0x000000bc   Code   RO         2634    i.UART_init         CVWL568.lib(drv_uart.o)
    0x00011228   0x00011228   0x00000018   Code   RO         2213    i.VIDC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00011240   0x00011240   0x00000018   Code   RO         2214    i.VPRE_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00011258   0x00011258   0x00000018   Code   RO         2215    i.WDG_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00011270   0x00011270   0x00000020   Code   RO         2986    i.__0printf         mc_p.l(printfa.o)
    0x00011290   0x00011290   0x00000024   Code   RO         2992    i.__0vsprintf       mc_p.l(printfa.o)
    0x000112b4   0x000112b4   0x0000002e   Code   RO         3087    i.__ARM_clz         mf_p.l(depilogue.o)
    0x000112e2   0x000112e2   0x0000001a   Code   RO          792    i.__ARM_common_switch8  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000112fc   0x000112fc   0x00000018   Code   RO         1651    i.__NVIC_ClearPendingIRQ  CVWL568.lib(drv_spi_master.o)
    0x00011314   0x00011314   0x00000020   Code   RO         2032    i.__NVIC_DisableIRQ  CVWL568.lib(drv_rxbr.o)
    0x00011334   0x00011334   0x00000018   Code   RO         2033    i.__NVIC_EnableIRQ  CVWL568.lib(drv_rxbr.o)
    0x0001134c   0x0001134c   0x00000044   Code   RO         2334    i.__NVIC_SetPriority  CVWL568.lib(hal_spi_slave.o)
    0x00011390   0x00011390   0x0000000e   Code   RO         3101    i.__scatterload_zeroinit  mc_p.l(handlers.o)
    0x0001139e   0x0001139e   0x00000002   PAD
    0x000113a0   0x000113a0   0x0000000c   Code   RO         3077    i.__set_errno       mc_p.l(errno.o)
    0x000113ac   0x000113ac   0x00000174   Code   RO         2993    i._fp_digits        mc_p.l(printfa.o)
    0x00011520   0x00011520   0x000006ec   Code   RO         2994    i._printf_core      mc_p.l(printfa.o)
    0x00011c0c   0x00011c0c   0x00000020   Code   RO         2995    i._printf_post_padding  mc_p.l(printfa.o)
    0x00011c2c   0x00011c2c   0x0000002c   Code   RO         2996    i._printf_pre_padding  mc_p.l(printfa.o)
    0x00011c58   0x00011c58   0x0000000a   Code   RO         2998    i._sputc            mc_p.l(printfa.o)
    0x00011c62   0x00011c62   0x00000002   PAD
    0x00011c64   0x00011c64   0x00001078   Code   RO          104    i.ap_dcs_read       ap_demo.o
    0x00012cdc   0x00012cdc   0x00000120   Code   RO          105    i.ap_demo           ap_demo.o
    0x00012dfc   0x00012dfc   0x0000004c   Code   RO          106    i.ap_get_reg_df     ap_demo.o
    0x00012e48   0x00012e48   0x00000020   Code   RO          418    i.ap_get_tp_calibration_status_01  app_tp_st_touch.o
    0x00012e68   0x00012e68   0x00000074   Code   RO          107    i.ap_set_backlight_51  ap_demo.o
    0x00012edc   0x00012edc   0x00000044   Code   RO          108    i.ap_set_display_off  ap_demo.o
    0x00012f20   0x00012f20   0x00000038   Code   RO          109    i.ap_set_display_on  ap_demo.o
    0x00012f58   0x00012f58   0x00000080   Code   RO          110    i.ap_set_enter_sleep_mode  ap_demo.o
    0x00012fd8   0x00012fd8   0x00000070   Code   RO          111    i.ap_set_exit_sleep_mode  ap_demo.o
    0x00013048   0x00013048   0x00000030   Code   RO          112    i.ap_set_hbm_53     ap_demo.o
    0x00013078   0x00013078   0x00000028   Code   RO          113    i.ap_update_frame_rate  ap_demo.o
    0x000130a0   0x000130a0   0x0000001c   Code   RO         2034    i.app_ADC_IRQn_Handler  CVWL568.lib(drv_rxbr.o)
    0x000130bc   0x000130bc   0x00000024   Code   RO         1451    i.app_AP_NRESET_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x000130e0   0x000130e0   0x0000001c   Code   RO         1452    i.app_EXTI_INT0_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x000130fc   0x000130fc   0x0000001c   Code   RO         1453    i.app_EXTI_INT1_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00013118   0x00013118   0x0000001c   Code   RO         1454    i.app_EXTI_INT2_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00013134   0x00013134   0x0000001c   Code   RO         1455    i.app_EXTI_INT3_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00013150   0x00013150   0x0000001c   Code   RO         1456    i.app_EXTI_INT4_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x0001316c   0x0001316c   0x0000001c   Code   RO         1457    i.app_EXTI_INT5_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00013188   0x00013188   0x0000001c   Code   RO         1458    i.app_EXTI_INT6_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x000131a4   0x000131a4   0x0000001c   Code   RO         1459    i.app_EXTI_INT7_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x000131c0   0x000131c0   0x00000048   Code   RO         1198    i.app_HardFault_Handler  CVWL568.lib(drv_common.o)
    0x00013208   0x00013208   0x00000018   Code   RO         1562    i.app_I2C0_IRQn_Handler  CVWL568.lib(drv_i2c_slave.o)
    0x00013220   0x00013220   0x00000010   Code   RO         1528    i.app_I2C1_IRQn_Handler  CVWL568.lib(drv_i2c_master.o)
    0x00013230   0x00013230   0x00000130   Code   RO         1099    i.app_LCDC_IRQn_Handler  CVWL568.lib(hal_internal_vsync.o)
    0x00013360   0x00013360   0x00000088   Code   RO         1976    i.app_MEMC_IRQn_Handler  CVWL568.lib(drv_memc.o)
    0x000133e8   0x000133e8   0x00000298   Code   RO         1746    i.app_MIPI_RX_IRQn_Handler  CVWL568.lib(drv_dsi_rx.o)
    0x00013680   0x00013680   0x000000a0   Code   RO         1804    i.app_MIPI_TX_IRQn_Handler  CVWL568.lib(drv_dsi_tx.o)
    0x00013720   0x00013720   0x00000048   Code   RO         2488    i.app_PWMDET_IRQn_Handler  CVWL568.lib(drv_pwm.o)
    0x00013768   0x00013768   0x00000030   Code   RO         1652    i.app_SPIM_IRQn_Handler  CVWL568.lib(drv_spi_master.o)
    0x00013798   0x00013798   0x00000200   Code   RO         2335    i.app_SPIS_IRQn_Handler  CVWL568.lib(hal_spi_slave.o)
    0x00013998   0x00013998   0x00000020   Code   RO         2553    i.app_SWIRE_IRQn_Handler  CVWL568.lib(drv_swire.o)
    0x000139b8   0x000139b8   0x00000018   Code   RO         1199    i.app_SysTick_Handler  CVWL568.lib(drv_common.o)
    0x000139d0   0x000139d0   0x0000000a   Code   RO         2572    i.app_TIMER0_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x000139da   0x000139da   0x0000000a   Code   RO         2573    i.app_TIMER1_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x000139e4   0x000139e4   0x0000000a   Code   RO         2574    i.app_TIMER2_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x000139ee   0x000139ee   0x0000000a   Code   RO         2575    i.app_TIMER3_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x000139f8   0x000139f8   0x00000008   Code   RO         2635    i.app_UART_IRQn_Handler  CVWL568.lib(drv_uart.o)
    0x00013a00   0x00013a00   0x0000001c   Code   RO         2105    i.app_VIDC_IRQn_Handler  CVWL568.lib(drv_vidc.o)
    0x00013a1c   0x00013a1c   0x0000001c   Code   RO         2035    i.app_VPRE_IRQn_Handler  CVWL568.lib(drv_rxbr.o)
    0x00013a38   0x00013a38   0x00000038   Code   RO         2694    i.app_WDG_IRQn_Handler  CVWL568.lib(drv_wdg.o)
    0x00013a70   0x00013a70   0x00000010   Code   RO         1313    i.app_dma_irq_handler  CVWL568.lib(drv_dma.o)
    0x00013a80   0x00013a80   0x00000030   Code   RO         2377    i.app_fls_ctrl_Handler  CVWL568.lib(norflash.o)
    0x00013ab0   0x00013ab0   0x00000024   Code   RO          542    i.board_Init        board.o
    0x00013ad4   0x00013ad4   0x0000058c   Code   RO         1100    i.calc_framebuffer_setting  CVWL568.lib(hal_internal_vsync.o)
    0x00014060   0x00014060   0x000000c8   Code   RO         2729    i.ceil              m_ps.l(ceil.o)
    0x00014128   0x00014128   0x0000002c   Code   RO         1101    i.check_mipi_rx_tx_video_info  CVWL568.lib(hal_internal_vsync.o)
    0x00014154   0x00014154   0x00000084   Code   RO         1102    i.check_pkt_buf_rev  CVWL568.lib(hal_internal_vsync.o)
    0x000141d8   0x000141d8   0x00000058   Code   RO         2717    i.dcs_packet_fifo_alloc  CVWL568.lib(dcs_packet_fifo.o)
    0x00014230   0x00014230   0x00000018   Code   RO         2718    i.dcs_packet_fifo_init  CVWL568.lib(dcs_packet_fifo.o)
    0x00014248   0x00014248   0x00000044   Code   RO         2719    i.dcs_packet_free_fifo_header  CVWL568.lib(dcs_packet_fifo.o)
    0x0001428c   0x0001428c   0x00000024   Code   RO         2720    i.dcs_packet_get_fifo_header  CVWL568.lib(dcs_packet_fifo.o)
    0x000142b0   0x000142b0   0x0000002c   Code   RO         1103    i.dcs_sw_filter     CVWL568.lib(hal_internal_vsync.o)
    0x000142dc   0x000142dc   0x00000018   Code   RO         1061    i.delayMs           CVWL568.lib(tau_delay.o)
    0x000142f4   0x000142f4   0x00000022   Code   RO         1062    i.delayUs           CVWL568.lib(tau_delay.o)
    0x00014316   0x00014316   0x00000002   PAD
    0x00014318   0x00014318   0x00000038   Code   RO         1684    i.drv_ap_rst_trig_edge_detect  CVWL568.lib(drv_sys_cfg.o)
    0x00014350   0x00014350   0x0000000c   Code   RO         2305    i.drv_chip_info_get_info  CVWL568.lib(drv_chip_info.o)
    0x0001435c   0x0001435c   0x00000040   Code   RO         2306    i.drv_chip_info_init  CVWL568.lib(drv_chip_info.o)
    0x0001439c   0x0001439c   0x000000b0   Code   RO         2307    i.drv_chip_rx_info_check  CVWL568.lib(drv_chip_info.o)
    0x0001444c   0x0001444c   0x00000014   Code   RO         2308    i.drv_chip_rx_init_done  CVWL568.lib(drv_chip_info.o)
    0x00014460   0x00014460   0x00000058   Code   RO         1201    i.drv_common_enable_systick  CVWL568.lib(drv_common.o)
    0x000144b8   0x000144b8   0x00000008   Code   RO         1204    i.drv_common_system_init  CVWL568.lib(drv_common.o)
    0x000144c0   0x000144c0   0x00000010   Code   RO         1226    i.drv_crgu_config_reset_modules  CVWL568.lib(drv_crgu.o)
    0x000144d0   0x000144d0   0x00000014   Code   RO         1239    i.drv_crgu_set_ahb_pre_div  CVWL568.lib(drv_crgu.o)
    0x000144e4   0x000144e4   0x00000014   Code   RO         1240    i.drv_crgu_set_ahb_src  CVWL568.lib(drv_crgu.o)
    0x000144f8   0x000144f8   0x00000020   Code   RO         1243    i.drv_crgu_set_clock  CVWL568.lib(drv_crgu.o)
    0x00014518   0x00014518   0x00000014   Code   RO         1244    i.drv_crgu_set_dpi_mux_src  CVWL568.lib(drv_crgu.o)
    0x0001452c   0x0001452c   0x00000018   Code   RO         1245    i.drv_crgu_set_dpi_pre_div  CVWL568.lib(drv_crgu.o)
    0x00014544   0x00014544   0x00000014   Code   RO         1246    i.drv_crgu_set_dpi_pre_src  CVWL568.lib(drv_crgu.o)
    0x00014558   0x00014558   0x00000014   Code   RO         1247    i.drv_crgu_set_dsc_core_div  CVWL568.lib(drv_crgu.o)
    0x0001456c   0x0001456c   0x00000014   Code   RO         1248    i.drv_crgu_set_dsco_src  CVWL568.lib(drv_crgu.o)
    0x00014580   0x00014580   0x00000014   Code   RO         1249    i.drv_crgu_set_dsco_src_div  CVWL568.lib(drv_crgu.o)
    0x00014594   0x00014594   0x00000014   Code   RO         1250    i.drv_crgu_set_fb_div  CVWL568.lib(drv_crgu.o)
    0x000145a8   0x000145a8   0x00000014   Code   RO         1251    i.drv_crgu_set_fb_src  CVWL568.lib(drv_crgu.o)
    0x000145bc   0x000145bc   0x00000014   Code   RO         1254    i.drv_crgu_set_lcdc_div  CVWL568.lib(drv_crgu.o)
    0x000145d0   0x000145d0   0x00000014   Code   RO         1255    i.drv_crgu_set_lcdc_src  CVWL568.lib(drv_crgu.o)
    0x000145e4   0x000145e4   0x00000014   Code   RO         1256    i.drv_crgu_set_mipi_cfg_src  CVWL568.lib(drv_crgu.o)
    0x000145f8   0x000145f8   0x00000018   Code   RO         1257    i.drv_crgu_set_mipi_ref_src  CVWL568.lib(drv_crgu.o)
    0x00014610   0x00014610   0x00000018   Code   RO         1260    i.drv_crgu_set_reset  CVWL568.lib(drv_crgu.o)
    0x00014628   0x00014628   0x00000014   Code   RO         1261    i.drv_crgu_set_rxbr_div  CVWL568.lib(drv_crgu.o)
    0x0001463c   0x0001463c   0x00000014   Code   RO         1262    i.drv_crgu_set_rxbr_src  CVWL568.lib(drv_crgu.o)
    0x00014650   0x00014650   0x00000014   Code   RO         1264    i.drv_crgu_set_vidc_src  CVWL568.lib(drv_crgu.o)
    0x00014664   0x00014664   0x00000018   Code   RO         1317    i.drv_dma_clear_flag  CVWL568.lib(drv_dma.o)
    0x0001467c   0x0001467c   0x0000000c   Code   RO         1325    i.drv_dma_get_channel_flag  CVWL568.lib(drv_dma.o)
    0x00014688   0x00014688   0x00000090   Code   RO         1328    i.drv_dma_irq_handler  CVWL568.lib(drv_dma.o)
    0x00014718   0x00014718   0x00000036   Code   RO         2318    i.drv_dsc_dec_convert_pps_rc_parameter  CVWL568.lib(drv_dsc_dec.o)
    0x0001474e   0x0001474e   0x0000000c   Code   RO         2319    i.drv_dsc_dec_disable  CVWL568.lib(drv_dsc_dec.o)
    0x0001475a   0x0001475a   0x00000002   PAD
    0x0001475c   0x0001475c   0x00000074   Code   RO         2320    i.drv_dsc_dec_enable  CVWL568.lib(drv_dsc_dec.o)
    0x000147d0   0x000147d0   0x0000000a   Code   RO         2321    i.drv_dsc_dec_get_nslc  CVWL568.lib(drv_dsc_dec.o)
    0x000147da   0x000147da   0x00000028   Code   RO         2323    i.drv_dsc_dec_set_u8_pps  CVWL568.lib(drv_dsc_dec.o)
    0x00014802   0x00014802   0x00000002   PAD
    0x00014804   0x00014804   0x00000104   Code   RO         1747    i.drv_dsi_rx_calc_ipi_tx_delay  CVWL568.lib(drv_dsi_rx.o)
    0x00014908   0x00014908   0x00000040   Code   RO         1748    i.drv_dsi_rx_enable_irq  CVWL568.lib(drv_dsi_rx.o)
    0x00014948   0x00014948   0x0000000e   Code   RO         1749    i.drv_dsi_rx_get_bta_status  CVWL568.lib(drv_dsi_rx.o)
    0x00014956   0x00014956   0x00000002   PAD
    0x00014958   0x00014958   0x00000050   Code   RO         1750    i.drv_dsi_rx_get_color_bpp  CVWL568.lib(drv_dsi_rx.o)
    0x000149a8   0x000149a8   0x0000001c   Code   RO         1751    i.drv_dsi_rx_get_color_pcc  CVWL568.lib(drv_dsi_rx.o)
    0x000149c4   0x000149c4   0x00000008   Code   RO         1752    i.drv_dsi_rx_get_compression_en  CVWL568.lib(drv_dsi_rx.o)
    0x000149cc   0x000149cc   0x00000006   Code   RO         1753    i.drv_dsi_rx_get_max_ret_size  CVWL568.lib(drv_dsi_rx.o)
    0x000149d2   0x000149d2   0x0000000e   Code   RO         1757    i.drv_dsi_rx_power_up  CVWL568.lib(drv_dsi_rx.o)
    0x000149e0   0x000149e0   0x00000020   Code   RO         1758    i.drv_dsi_rx_set_ctrl_cfg  CVWL568.lib(drv_dsi_rx.o)
    0x00014a00   0x00014a00   0x00000010   Code   RO         1759    i.drv_dsi_rx_set_ddi_cfg  CVWL568.lib(drv_dsi_rx.o)
    0x00014a10   0x00014a10   0x00000004   Code   RO         1761    i.drv_dsi_rx_set_inten  CVWL568.lib(drv_dsi_rx.o)
    0x00014a14   0x00014a14   0x00000010   Code   RO         1762    i.drv_dsi_rx_set_ipi_cfg  CVWL568.lib(drv_dsi_rx.o)
    0x00014a24   0x00014a24   0x00000046   Code   RO         1764    i.drv_dsi_rx_set_lane_swap  CVWL568.lib(drv_dsi_rx.o)
    0x00014a6a   0x00014a6a   0x00000026   Code   RO         1765    i.drv_dsi_rx_set_resp_cnt  CVWL568.lib(drv_dsi_rx.o)
    0x00014a90   0x00014a90   0x00000104   Code   RO         1766    i.drv_dsi_rx_set_up_phy  CVWL568.lib(drv_dsi_rx.o)
    0x00014b94   0x00014b94   0x0000000e   Code   RO         1767    i.drv_dsi_rx_shut_down  CVWL568.lib(drv_dsi_rx.o)
    0x00014ba2   0x00014ba2   0x00000014   Code   RO         1806    i.drv_dsi_tx_command_header  CVWL568.lib(drv_dsi_tx.o)
    0x00014bb6   0x00014bb6   0x0000006c   Code   RO         1807    i.drv_dsi_tx_command_mode_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x00014c22   0x00014c22   0x00000004   Code   RO         1808    i.drv_dsi_tx_command_put_payload  CVWL568.lib(drv_dsi_tx.o)
    0x00014c26   0x00014c26   0x00000018   Code   RO         1809    i.drv_dsi_tx_config_eotp  CVWL568.lib(drv_dsi_tx.o)
    0x00014c3e   0x00014c3e   0x00000008   Code   RO         1810    i.drv_dsi_tx_config_int  CVWL568.lib(drv_dsi_tx.o)
    0x00014c46   0x00014c46   0x00000008   Code   RO         1811    i.drv_dsi_tx_dpi_lpcmd_time  CVWL568.lib(drv_dsi_tx.o)
    0x00014c4e   0x00014c4e   0x0000000a   Code   RO         1812    i.drv_dsi_tx_dpi_mode  CVWL568.lib(drv_dsi_tx.o)
    0x00014c58   0x00014c58   0x00000024   Code   RO         1813    i.drv_dsi_tx_dpi_polarity  CVWL568.lib(drv_dsi_tx.o)
    0x00014c7c   0x00014c7c   0x00000004   Code   RO         1814    i.drv_dsi_tx_edpi_cmd_size  CVWL568.lib(drv_dsi_tx.o)
    0x00014c80   0x00014c80   0x00000004   Code   RO         1816    i.drv_dsi_tx_get_cmd_status  CVWL568.lib(drv_dsi_tx.o)
    0x00014c84   0x00014c84   0x00000004   Code   RO         1818    i.drv_dsi_tx_mode   CVWL568.lib(drv_dsi_tx.o)
    0x00014c88   0x00014c88   0x00000018   Code   RO         1819    i.drv_dsi_tx_phy_clock_lane_auto_lp  CVWL568.lib(drv_dsi_tx.o)
    0x00014ca0   0x00014ca0   0x0000001a   Code   RO         1820    i.drv_dsi_tx_phy_clock_lane_req_hs  CVWL568.lib(drv_dsi_tx.o)
    0x00014cba   0x00014cba   0x0000000c   Code   RO         1822    i.drv_dsi_tx_phy_lane_mode  CVWL568.lib(drv_dsi_tx.o)
    0x00014cc6   0x00014cc6   0x00000064   Code   RO         1826    i.drv_dsi_tx_phy_status_ready  CVWL568.lib(drv_dsi_tx.o)
    0x00014d2a   0x00014d2a   0x0000003e   Code   RO         1827    i.drv_dsi_tx_phy_status_stopstate  CVWL568.lib(drv_dsi_tx.o)
    0x00014d68   0x00014d68   0x00000134   Code   RO         1829    i.drv_dsi_tx_phy_test_setup  CVWL568.lib(drv_dsi_tx.o)
    0x00014e9c   0x00014e9c   0x0000001e   Code   RO         1830    i.drv_dsi_tx_phy_time_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x00014eba   0x00014eba   0x00000008   Code   RO         1834    i.drv_dsi_tx_powerup  CVWL568.lib(drv_dsi_tx.o)
    0x00014ec2   0x00014ec2   0x0000001c   Code   RO         1835    i.drv_dsi_tx_response_mode  CVWL568.lib(drv_dsi_tx.o)
    0x00014ede   0x00014ede   0x00000018   Code   RO         1838    i.drv_dsi_tx_set_bta_ack  CVWL568.lib(drv_dsi_tx.o)
    0x00014ef6   0x00014ef6   0x0000000c   Code   RO         1839    i.drv_dsi_tx_set_esc_div  CVWL568.lib(drv_dsi_tx.o)
    0x00014f02   0x00014f02   0x00000002   PAD
    0x00014f04   0x00014f04   0x00000040   Code   RO         1840    i.drv_dsi_tx_set_int  CVWL568.lib(drv_dsi_tx.o)
    0x00014f44   0x00014f44   0x00000010   Code   RO         1841    i.drv_dsi_tx_set_time_out_div  CVWL568.lib(drv_dsi_tx.o)
    0x00014f54   0x00014f54   0x00000008   Code   RO         1842    i.drv_dsi_tx_set_video_chunk  CVWL568.lib(drv_dsi_tx.o)
    0x00014f5c   0x00014f5c   0x00000022   Code   RO         1843    i.drv_dsi_tx_set_video_timing  CVWL568.lib(drv_dsi_tx.o)
    0x00014f7e   0x00014f7e   0x00000008   Code   RO         1845    i.drv_dsi_tx_shutdown  CVWL568.lib(drv_dsi_tx.o)
    0x00014f86   0x00014f86   0x00000026   Code   RO         1846    i.drv_dsi_tx_timeout_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x00014fac   0x00014fac   0x000000aa   Code   RO         1849    i.drv_dsi_tx_video_mode_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x00015056   0x00015056   0x00000016   Code   RO         1850    i.drv_dsi_tx_video_mode_disable_hact_cmd  CVWL568.lib(drv_dsi_tx.o)
    0x0001506c   0x0001506c   0x00000018   Code   RO         1851    i.drv_dsi_tx_video_mode_set_lp_cmd  CVWL568.lib(drv_dsi_tx.o)
    0x00015084   0x00015084   0x0000002e   Code   RO         2256    i.drv_efuse_enter_inactive  CVWL568.lib(drv_efuse.o)
    0x000150b2   0x000150b2   0x0000000c   Code   RO         2259    i.drv_efuse_int_enable  CVWL568.lib(drv_efuse.o)
    0x000150be   0x000150be   0x00000032   Code   RO         2260    i.drv_efuse_read    CVWL568.lib(drv_efuse.o)
    0x000150f0   0x000150f0   0x00000018   Code   RO         2261    i.drv_efuse_read_req  CVWL568.lib(drv_efuse.o)
    0x00015108   0x00015108   0x00000020   Code   RO         1466    i.drv_gpio_set_ioe  CVWL568.lib(drv_gpio.o)
    0x00015128   0x00015128   0x00000010   Code   RO         1467    i.drv_gpio_set_mode0  CVWL568.lib(drv_gpio.o)
    0x00015138   0x00015138   0x00000010   Code   RO         1468    i.drv_gpio_set_mode1  CVWL568.lib(drv_gpio.o)
    0x00015148   0x00015148   0x00000010   Code   RO         1469    i.drv_gpio_set_mode2  CVWL568.lib(drv_gpio.o)
    0x00015158   0x00015158   0x00000010   Code   RO         1470    i.drv_gpio_set_mode3  CVWL568.lib(drv_gpio.o)
    0x00015168   0x00015168   0x00000020   Code   RO          902    i.drv_gpio_set_output_data  CVWL568.lib(hal_gpio.o)
    0x00015188   0x00015188   0x00000018   Code   RO         1918    i.drv_lcdc_config_bypass  CVWL568.lib(drv_lcdc.o)
    0x000151a0   0x000151a0   0x00000030   Code   RO         1919    i.drv_lcdc_config_ccm  CVWL568.lib(drv_lcdc.o)
    0x000151d0   0x000151d0   0x00000016   Code   RO         1920    i.drv_lcdc_config_disp_mode  CVWL568.lib(drv_lcdc.o)
    0x000151e6   0x000151e6   0x00000024   Code   RO         1921    i.drv_lcdc_config_dpi_polarity  CVWL568.lib(drv_lcdc.o)
    0x0001520a   0x0001520a   0x00000026   Code   RO         1922    i.drv_lcdc_config_dpi_timing  CVWL568.lib(drv_lcdc.o)
    0x00015230   0x00015230   0x00000016   Code   RO         1923    i.drv_lcdc_config_edpi_mode  CVWL568.lib(drv_lcdc.o)
    0x00015246   0x00015246   0x00000016   Code   RO         1924    i.drv_lcdc_config_endianness  CVWL568.lib(drv_lcdc.o)
    0x0001525c   0x0001525c   0x0000000c   Code   RO         1925    i.drv_lcdc_config_input_size  CVWL568.lib(drv_lcdc.o)
    0x00015268   0x00015268   0x0000001e   Code   RO         1926    i.drv_lcdc_config_int  CVWL568.lib(drv_lcdc.o)
    0x00015286   0x00015286   0x00000022   Code   RO         1927    i.drv_lcdc_config_int_single  CVWL568.lib(drv_lcdc.o)
    0x000152a8   0x000152a8   0x00000022   Code   RO         1928    i.drv_lcdc_config_overwrite  CVWL568.lib(drv_lcdc.o)
    0x000152ca   0x000152ca   0x0000000c   Code   RO         1929    i.drv_lcdc_config_overwrite_rgb  CVWL568.lib(drv_lcdc.o)
    0x000152d6   0x000152d6   0x0000001a   Code   RO         1930    i.drv_lcdc_config_partial_display_area  CVWL568.lib(drv_lcdc.o)
    0x000152f0   0x000152f0   0x00000022   Code   RO         1931    i.drv_lcdc_config_partial_display_enable  CVWL568.lib(drv_lcdc.o)
    0x00015312   0x00015312   0x0000001a   Code   RO         1933    i.drv_lcdc_config_scale_up_coef  CVWL568.lib(drv_lcdc.o)
    0x0001532c   0x0001532c   0x0000000c   Code   RO         1934    i.drv_lcdc_config_scale_up_step  CVWL568.lib(drv_lcdc.o)
    0x00015338   0x00015338   0x0000004c   Code   RO         1935    i.drv_lcdc_config_src_parameter  CVWL568.lib(drv_lcdc.o)
    0x00015384   0x00015384   0x00000006   Code   RO         1936    i.drv_lcdc_config_thresh  CVWL568.lib(drv_lcdc.o)
    0x0001538a   0x0001538a   0x00000012   Code   RO         1937    i.drv_lcdc_ctrl_flow  CVWL568.lib(drv_lcdc.o)
    0x0001539c   0x0001539c   0x00000020   Code   RO         1939    i.drv_lcdc_enable_shadow_reg  CVWL568.lib(drv_lcdc.o)
    0x000153bc   0x000153bc   0x00000040   Code   RO         1940    i.drv_lcdc_set_int  CVWL568.lib(drv_lcdc.o)
    0x000153fc   0x000153fc   0x00000018   Code   RO         1941    i.drv_lcdc_set_prefetch  CVWL568.lib(drv_lcdc.o)
    0x00015414   0x00015414   0x00000014   Code   RO         1942    i.drv_lcdc_set_video_hw_mode  CVWL568.lib(drv_lcdc.o)
    0x00015428   0x00015428   0x00000020   Code   RO         1943    i.drv_lcdc_start    CVWL568.lib(drv_lcdc.o)
    0x00015448   0x00015448   0x0000000c   Code   RO         1977    i.drv_memc_clear_status  CVWL568.lib(drv_memc.o)
    0x00015454   0x00015454   0x00000040   Code   RO         1978    i.drv_memc_enable_irq  CVWL568.lib(drv_memc.o)
    0x00015494   0x00015494   0x0000000c   Code   RO         1979    i.drv_memc_gen_a_tear_signal  CVWL568.lib(drv_memc.o)
    0x000154a0   0x000154a0   0x00000012   Code   RO         1980    i.drv_memc_get_status  CVWL568.lib(drv_memc.o)
    0x000154b2   0x000154b2   0x00000010   Code   RO         1981    i.drv_memc_rate_transfer_sel  CVWL568.lib(drv_memc.o)
    0x000154c2   0x000154c2   0x0000000e   Code   RO         1982    i.drv_memc_sel_vsync  CVWL568.lib(drv_memc.o)
    0x000154d0   0x000154d0   0x00000014   Code   RO         1983    i.drv_memc_set_active_height  CVWL568.lib(drv_memc.o)
    0x000154e4   0x000154e4   0x0000000c   Code   RO         1984    i.drv_memc_set_data_mode  CVWL568.lib(drv_memc.o)
    0x000154f0   0x000154f0   0x00000010   Code   RO         1987    i.drv_memc_set_double_buffer  CVWL568.lib(drv_memc.o)
    0x00015500   0x00015500   0x00000012   Code   RO         1988    i.drv_memc_set_double_buffer_reverse  CVWL568.lib(drv_memc.o)
    0x00015512   0x00015512   0x00000010   Code   RO         1990    i.drv_memc_set_fs_en_conditions  CVWL568.lib(drv_memc.o)
    0x00015522   0x00015522   0x00000014   Code   RO         1991    i.drv_memc_set_inten  CVWL568.lib(drv_memc.o)
    0x00015536   0x00015536   0x00000002   PAD
    0x00015538   0x00015538   0x00000018   Code   RO         1992    i.drv_memc_set_lcdc_st_conditions  CVWL568.lib(drv_memc.o)
    0x00015550   0x00015550   0x0000001a   Code   RO         1993    i.drv_memc_set_ltpo_mode  CVWL568.lib(drv_memc.o)
    0x0001556a   0x0001556a   0x0000000e   Code   RO         1997    i.drv_memc_set_tear_mode  CVWL568.lib(drv_memc.o)
    0x00015578   0x00015578   0x00000028   Code   RO         1998    i.drv_memc_set_tear_waveform  CVWL568.lib(drv_memc.o)
    0x000155a0   0x000155a0   0x0000000e   Code   RO         2000    i.drv_memc_set_vidc_sync_cnt  CVWL568.lib(drv_memc.o)
    0x000155ae   0x000155ae   0x00000002   PAD
    0x000155b0   0x000155b0   0x00000008   Code   RO         1589    i.drv_param_init_get_ccm  CVWL568.lib(drv_param_init.o)
    0x000155b8   0x000155b8   0x00000014   Code   RO         1590    i.drv_param_init_get_scld_filter_h  CVWL568.lib(drv_param_init.o)
    0x000155cc   0x000155cc   0x00000014   Code   RO         1591    i.drv_param_init_get_scld_filter_v  CVWL568.lib(drv_param_init.o)
    0x000155e0   0x000155e0   0x00000008   Code   RO         1592    i.drv_param_init_get_sclu_filter  CVWL568.lib(drv_param_init.o)
    0x000155e8   0x000155e8   0x00000014   Code   RO         1593    i.drv_param_init_set_ccm  CVWL568.lib(drv_param_init.o)
    0x000155fc   0x000155fc   0x00000064   Code   RO         1594    i.drv_param_init_set_scld_filter  CVWL568.lib(drv_param_init.o)
    0x00015660   0x00015660   0x00000024   Code   RO         1596    i.drv_param_p2r_filter_init  CVWL568.lib(drv_param_init.o)
    0x00015684   0x00015684   0x00000010   Code   RO         2277    i.drv_phy_enable_calibration  CVWL568.lib(drv_phy_common.o)
    0x00015694   0x00015694   0x0000003c   Code   RO         2278    i.drv_phy_get_calibration  CVWL568.lib(drv_phy_common.o)
    0x000156d0   0x000156d0   0x00000060   Code   RO         2279    i.drv_phy_get_pll_para  CVWL568.lib(drv_phy_common.o)
    0x00015730   0x00015730   0x00000054   Code   RO         2280    i.drv_phy_get_rate_para  CVWL568.lib(drv_phy_common.o)
    0x00015784   0x00015784   0x00000010   Code   RO         2281    i.drv_phy_test_clear  CVWL568.lib(drv_phy_common.o)
    0x00015794   0x00015794   0x00000018   Code   RO         2282    i.drv_phy_test_lock  CVWL568.lib(drv_phy_common.o)
    0x000157ac   0x000157ac   0x00000020   Code   RO         2284    i.drv_phy_test_write_1_byte  CVWL568.lib(drv_phy_common.o)
    0x000157cc   0x000157cc   0x00000026   Code   RO         2285    i.drv_phy_test_write_2_byte  CVWL568.lib(drv_phy_common.o)
    0x000157f2   0x000157f2   0x0000001e   Code   RO         2286    i.drv_phy_test_write_code  CVWL568.lib(drv_phy_common.o)
    0x00015810   0x00015810   0x00000020   Code   RO         2287    i.drv_phy_test_write_data  CVWL568.lib(drv_phy_common.o)
    0x00015830   0x00015830   0x00000018   Code   RO         1614    i.drv_pwr_set_pvd_mode  CVWL568.lib(drv_pwr.o)
    0x00015848   0x00015848   0x00000038   Code   RO         1615    i.drv_pwr_set_system_clk_src  CVWL568.lib(drv_pwr.o)
    0x00015880   0x00015880   0x0000000c   Code   RO         1768    i.drv_rx_phy_test_clear  CVWL568.lib(drv_dsi_rx.o)
    0x0001588c   0x0001588c   0x00000010   Code   RO         1769    i.drv_rx_phy_test_lock  CVWL568.lib(drv_dsi_rx.o)
    0x0001589c   0x0001589c   0x00000014   Code   RO         1771    i.drv_rx_phy_test_write_1_byte  CVWL568.lib(drv_dsi_rx.o)
    0x000158b0   0x000158b0   0x00000016   Code   RO         1772    i.drv_rx_phy_test_write_2_byte  CVWL568.lib(drv_dsi_rx.o)
    0x000158c6   0x000158c6   0x0000000a   Code   RO         2036    i.drv_rxbr_clear_pkt_buffer  CVWL568.lib(drv_rxbr.o)
    0x000158d0   0x000158d0   0x00000004   Code   RO         2037    i.drv_rxbr_clear_status0  CVWL568.lib(drv_rxbr.o)
    0x000158d4   0x000158d4   0x0000005a   Code   RO         2039    i.drv_rxbr_enable_irq  CVWL568.lib(drv_rxbr.o)
    0x0001592e   0x0001592e   0x00000002   PAD
    0x00015930   0x00015930   0x00000014   Code   RO         2040    i.drv_rxbr_frame_drop_cfg  CVWL568.lib(drv_rxbr.o)
    0x00015944   0x00015944   0x00000064   Code   RO         2041    i.drv_rxbr_get_clk  CVWL568.lib(drv_rxbr.o)
    0x000159a8   0x000159a8   0x00000004   Code   RO         2042    i.drv_rxbr_get_col_addr  CVWL568.lib(drv_rxbr.o)
    0x000159ac   0x000159ac   0x00000012   Code   RO         1104    i.drv_rxbr_get_int_source  CVWL568.lib(hal_internal_vsync.o)
    0x000159be   0x000159be   0x00000004   Code   RO         2045    i.drv_rxbr_get_page_addr  CVWL568.lib(drv_rxbr.o)
    0x000159c2   0x000159c2   0x0000000c   Code   RO         2047    i.drv_rxbr_get_pkt_buf_error_status  CVWL568.lib(drv_rxbr.o)
    0x000159ce   0x000159ce   0x00000012   Code   RO         1105    i.drv_rxbr_get_status0  CVWL568.lib(hal_internal_vsync.o)
    0x000159e0   0x000159e0   0x00000016   Code   RO         1106    i.drv_rxbr_get_status1  CVWL568.lib(hal_internal_vsync.o)
    0x000159f6   0x000159f6   0x0000000c   Code   RO         2048    i.drv_rxbr_hline_rcv0_cfg  CVWL568.lib(drv_rxbr.o)
    0x00015a02   0x00015a02   0x0000000c   Code   RO         2049    i.drv_rxbr_hline_rcv1_cfg  CVWL568.lib(drv_rxbr.o)
    0x00015a0e   0x00015a0e   0x00000008   Code   RO         2050    i.drv_rxbr_hline_rcv_cfg  CVWL568.lib(drv_rxbr.o)
    0x00015a16   0x00015a16   0x00000002   PAD
    0x00015a18   0x00015a18   0x0000000c   Code   RO         2051    i.drv_rxbr_register_irq0_callback  CVWL568.lib(drv_rxbr.o)
    0x00015a24   0x00015a24   0x0000000c   Code   RO         2052    i.drv_rxbr_register_irq1_callback  CVWL568.lib(drv_rxbr.o)
    0x00015a30   0x00015a30   0x00000014   Code   RO         2053    i.drv_rxbr_set_ack_pkt_header  CVWL568.lib(drv_rxbr.o)
    0x00015a44   0x00015a44   0x00000014   Code   RO         2056    i.drv_rxbr_set_color_format  CVWL568.lib(drv_rxbr.o)
    0x00015a58   0x00015a58   0x00000012   Code   RO         2058    i.drv_rxbr_set_filter_regs  CVWL568.lib(drv_rxbr.o)
    0x00015a6a   0x00015a6a   0x00000014   Code   RO         2059    i.drv_rxbr_set_inten  CVWL568.lib(drv_rxbr.o)
    0x00015a7e   0x00015a7e   0x00000010   Code   RO         2060    i.drv_rxbr_set_ltpo_drop_th  CVWL568.lib(drv_rxbr.o)
    0x00015a8e   0x00015a8e   0x00000026   Code   RO         2062    i.drv_rxbr_set_usr_cfg  CVWL568.lib(drv_rxbr.o)
    0x00015ab4   0x00015ab4   0x00000008   Code   RO         2063    i.drv_rxbr_set_usr_col  CVWL568.lib(drv_rxbr.o)
    0x00015abc   0x00015abc   0x00000008   Code   RO         2064    i.drv_rxbr_set_usr_row  CVWL568.lib(drv_rxbr.o)
    0x00015ac4   0x00015ac4   0x00000054   Code   RO         2557    i.drv_swire_set_int  CVWL568.lib(drv_swire.o)
    0x00015b18   0x00015b18   0x0000000c   Code   RO         1685    i.drv_sys_cfg_clear_all_int  CVWL568.lib(drv_sys_cfg.o)
    0x00015b24   0x00015b24   0x00000028   Code   RO         1686    i.drv_sys_cfg_clear_pending  CVWL568.lib(drv_sys_cfg.o)
    0x00015b4c   0x00015b4c   0x00000018   Code   RO         1689    i.drv_sys_cfg_sel_ap_rst_lvl_trig  CVWL568.lib(drv_sys_cfg.o)
    0x00015b64   0x00015b64   0x00000024   Code   RO         1696    i.drv_sys_cfg_set_int  CVWL568.lib(drv_sys_cfg.o)
    0x00015b88   0x00015b88   0x0000001a   Code   RO         2576    i.drv_timer_clear_status_flags  CVWL568.lib(drv_timer.o)
    0x00015ba2   0x00015ba2   0x00000020   Code   RO         2577    i.drv_timer_enable  CVWL568.lib(drv_timer.o)
    0x00015bc2   0x00015bc2   0x00000002   PAD
    0x00015bc4   0x00015bc4   0x00000010   Code   RO         2578    i.drv_timer_get_instance  CVWL568.lib(drv_timer.o)
    0x00015bd4   0x00015bd4   0x00000044   Code   RO         2581    i.drv_timer_handle_interrupt  CVWL568.lib(drv_timer.o)
    0x00015c18   0x00015c18   0x00000010   Code   RO         2583    i.drv_timer_set_compare_val  CVWL568.lib(drv_timer.o)
    0x00015c28   0x00015c28   0x00000054   Code   RO         2584    i.drv_timer_set_int  CVWL568.lib(drv_timer.o)
    0x00015c7c   0x00015c7c   0x0000000a   Code   RO         1852    i.drv_tx_phy_test_clear  CVWL568.lib(drv_dsi_tx.o)
    0x00015c86   0x00015c86   0x0000001c   Code   RO         1853    i.drv_tx_phy_test_enter  CVWL568.lib(drv_dsi_tx.o)
    0x00015ca2   0x00015ca2   0x0000001c   Code   RO         1854    i.drv_tx_phy_test_exit  CVWL568.lib(drv_dsi_tx.o)
    0x00015cbe   0x00015cbe   0x00000012   Code   RO         1856    i.drv_tx_phy_test_write_1_byte  CVWL568.lib(drv_dsi_tx.o)
    0x00015cd0   0x00015cd0   0x00000014   Code   RO         1857    i.drv_tx_phy_test_write_2_byte  CVWL568.lib(drv_dsi_tx.o)
    0x00015ce4   0x00015ce4   0x00000010   Code   RO         1858    i.drv_tx_phy_test_write_code  CVWL568.lib(drv_dsi_tx.o)
    0x00015cf4   0x00015cf4   0x00000008   Code   RO         2106    i.drv_vidc_clear_irq  CVWL568.lib(drv_vidc.o)
    0x00015cfc   0x00015cfc   0x00000018   Code   RO         2110    i.drv_vidc_enable   CVWL568.lib(drv_vidc.o)
    0x00015d14   0x00015d14   0x00000040   Code   RO         2111    i.drv_vidc_enable_irq  CVWL568.lib(drv_vidc.o)
    0x00015d54   0x00015d54   0x00000012   Code   RO         2113    i.drv_vidc_get_irq_status  CVWL568.lib(drv_vidc.o)
    0x00015d66   0x00015d66   0x00000002   PAD
    0x00015d68   0x00015d68   0x00000028   Code   RO         2117    i.drv_vidc_init_module_enable  CVWL568.lib(drv_vidc.o)
    0x00015d90   0x00015d90   0x0000000c   Code   RO         2118    i.drv_vidc_register_callback  CVWL568.lib(drv_vidc.o)
    0x00015d9c   0x00015d9c   0x00000006   Code   RO         2119    i.drv_vidc_reset    CVWL568.lib(drv_vidc.o)
    0x00015da2   0x00015da2   0x0000003c   Code   RO         2121    i.drv_vidc_set_dst_parameter  CVWL568.lib(drv_vidc.o)
    0x00015dde   0x00015dde   0x00000014   Code   RO         2125    i.drv_vidc_set_irqen  CVWL568.lib(drv_vidc.o)
    0x00015df2   0x00015df2   0x00000010   Code   RO         2126    i.drv_vidc_set_mirror  CVWL568.lib(drv_vidc.o)
    0x00015e02   0x00015e02   0x00000008   Code   RO         2129    i.drv_vidc_set_p2r_hcoef0  CVWL568.lib(drv_vidc.o)
    0x00015e0a   0x00015e0a   0x00000026   Code   RO         2130    i.drv_vidc_set_p2r_hinitb  CVWL568.lib(drv_vidc.o)
    0x00015e30   0x00015e30   0x00000026   Code   RO         2131    i.drv_vidc_set_p2r_hinitr  CVWL568.lib(drv_vidc.o)
    0x00015e56   0x00015e56   0x00000002   PAD
    0x00015e58   0x00015e58   0x00000018   Code   RO         2132    i.drv_vidc_set_pentile_swap  CVWL568.lib(drv_vidc.o)
    0x00015e70   0x00015e70   0x0000000a   Code   RO         2133    i.drv_vidc_set_pu_ctrl  CVWL568.lib(drv_vidc.o)
    0x00015e7a   0x00015e7a   0x00000010   Code   RO         2134    i.drv_vidc_set_rotation  CVWL568.lib(drv_vidc.o)
    0x00015e8a   0x00015e8a   0x0000000a   Code   RO         2135    i.drv_vidc_set_scld_hcoef0  CVWL568.lib(drv_vidc.o)
    0x00015e94   0x00015e94   0x0000000a   Code   RO         2136    i.drv_vidc_set_scld_hcoef1  CVWL568.lib(drv_vidc.o)
    0x00015e9e   0x00015e9e   0x00000012   Code   RO         2137    i.drv_vidc_set_scld_step  CVWL568.lib(drv_vidc.o)
    0x00015eb0   0x00015eb0   0x0000000a   Code   RO         2138    i.drv_vidc_set_scld_vcoef0  CVWL568.lib(drv_vidc.o)
    0x00015eba   0x00015eba   0x0000000a   Code   RO         2139    i.drv_vidc_set_scld_vcoef1  CVWL568.lib(drv_vidc.o)
    0x00015ec4   0x00015ec4   0x00000016   Code   RO         2140    i.drv_vidc_set_src_parameter  CVWL568.lib(drv_vidc.o)
    0x00015eda   0x00015eda   0x00000002   PAD
    0x00015edc   0x00015edc   0x00000010   Code   RO         2695    i.drv_wdg_clear_counter  CVWL568.lib(drv_wdg.o)
    0x00015eec   0x00015eec   0x00000010   Code   RO         2696    i.drv_wdg_clear_edge_flag  CVWL568.lib(drv_wdg.o)
    0x00015efc   0x00015efc   0x00000010   Code   RO         2699    i.drv_wdg_read_edge_flag  CVWL568.lib(drv_wdg.o)
    0x00015f0c   0x00015f0c   0x00000040   Code   RO         2702    i.drv_wdg_set_int   CVWL568.lib(drv_wdg.o)
    0x00015f4c   0x00015f4c   0x0000000a   Code   RO         1372    i.fls_clr_interrupt_flag  CVWL568.lib(drv_fls.o)
    0x00015f56   0x00015f56   0x00000014   Code   RO         1071    i.fputc             CVWL568.lib(tau_log.o)
    0x00015f6a   0x00015f6a   0x00000002   PAD
    0x00015f6c   0x00015f6c   0x00000050   Code   RO          114    i.frame_start_cb    ap_demo.o
    0x00015fbc   0x00015fbc   0x00000034   Code   RO          701    i.hal_dsi_rx_ctrl_create_handle  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00015ff0   0x00015ff0   0x00000028   Code   RO          705    i.hal_dsi_rx_ctrl_dsc_async_handler  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016018   0x00016018   0x00000028   Code   RO          707    i.hal_dsi_rx_ctrl_gen_a_tear_signal  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016040   0x00016040   0x00000028   Code   RO          709    i.hal_dsi_rx_ctrl_get_max_ret_size  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016068   0x00016068   0x00000098   Code   RO          711    i.hal_dsi_rx_ctrl_init  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016100   0x00016100   0x000001a4   Code   RO          712    i.hal_dsi_rx_ctrl_init_clk  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000162a4   0x000162a4   0x000000d8   Code   RO          713    i.hal_dsi_rx_ctrl_init_dsi_rx  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001637c   0x0001637c   0x00000160   Code   RO          714    i.hal_dsi_rx_ctrl_init_memc  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000164dc   0x000164dc   0x00000150   Code   RO          715    i.hal_dsi_rx_ctrl_init_rxbr  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001662c   0x0001662c   0x0000022c   Code   RO          716    i.hal_dsi_rx_ctrl_init_vidc  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016858   0x00016858   0x0000003c   Code   RO          717    i.hal_dsi_rx_ctrl_pre_init_pps  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016894   0x00016894   0x00000050   Code   RO          720    i.hal_dsi_rx_ctrl_restart  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000168e4   0x000168e4   0x000000f0   Code   RO          721    i.hal_dsi_rx_ctrl_send_ack_cmd  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000169d4   0x000169d4   0x0000002c   Code   RO          723    i.hal_dsi_rx_ctrl_set_cus_esc_clk  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016a00   0x00016a00   0x0000006c   Code   RO          724    i.hal_dsi_rx_ctrl_set_cus_scld_filter  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016a6c   0x00016a6c   0x00000034   Code   RO          725    i.hal_dsi_rx_ctrl_set_cus_sync_line  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016aa0   0x00016aa0   0x00000038   Code   RO          729    i.hal_dsi_rx_ctrl_set_ipi_cfg  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016ad8   0x00016ad8   0x00000072   Code   RO          734    i.hal_dsi_rx_ctrl_set_rxbr_clk  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016b4a   0x00016b4a   0x0000000e   Code   RO          737    i.hal_dsi_rx_ctrl_set_tear_mode_ex  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016b58   0x00016b58   0x0000003c   Code   RO          738    i.hal_dsi_rx_ctrl_start  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016b94   0x00016b94   0x00000020   Code   RO          741    i.hal_dsi_rx_ctrl_toggle_resolution  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016bb4   0x00016bb4   0x00000190   Code   RO          796    i.hal_dsi_tx_calc_video_chunks  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00016d44   0x00016d44   0x00000034   Code   RO          797    i.hal_dsi_tx_config_params_for_lane_rate  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00016d78   0x00016d78   0x00000428   Code   RO          798    i.hal_dsi_tx_count_lane_rate  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000171a0   0x000171a0   0x0000002c   Code   RO          801    i.hal_dsi_tx_ctrl_create_handle  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000171cc   0x000171cc   0x0000004c   Code   RO          806    i.hal_dsi_tx_ctrl_enter_init_panel_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017218   0x00017218   0x00000028   Code   RO          808    i.hal_dsi_tx_ctrl_exit_init_panel_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017240   0x00017240   0x000000a4   Code   RO          810    i.hal_dsi_tx_ctrl_init  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000172e4   0x000172e4   0x00000024   Code   RO          811    i.hal_dsi_tx_ctrl_init_clk  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017308   0x00017308   0x0000000c   Code   RO          812    i.hal_dsi_tx_ctrl_panel_reset_pin  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017314   0x00017314   0x00000020   Code   RO          815    i.hal_dsi_tx_ctrl_set_ccm  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017334   0x00017334   0x00000014   Code   RO          821    i.hal_dsi_tx_ctrl_set_overwrite_rgb  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017348   0x00017348   0x00000010   Code   RO          822    i.hal_dsi_tx_ctrl_set_partial_disp  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017358   0x00017358   0x00000024   Code   RO          823    i.hal_dsi_tx_ctrl_set_partial_disp_area  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001737c   0x0001737c   0x000000a8   Code   RO          826    i.hal_dsi_tx_ctrl_start  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017424   0x00017424   0x000000f0   Code   RO          828    i.hal_dsi_tx_ctrl_write_array_cmd  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017514   0x00017514   0x000000cc   Code   RO          829    i.hal_dsi_tx_ctrl_write_cmd  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000175e0   0x000175e0   0x00000044   Code   RO          830    i.hal_dsi_tx_init_data_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017624   0x00017624   0x00000030   Code   RO          831    i.hal_dsi_tx_init_dpi_cfg  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017654   0x00017654   0x00000020   Code   RO          832    i.hal_dsi_tx_init_interrupt  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017674   0x00017674   0x00000020   Code   RO          833    i.hal_dsi_tx_init_phy_cfg  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017694   0x00017694   0x00000094   Code   RO          834    i.hal_dsi_tx_init_remains  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017728   0x00017728   0x00000058   Code   RO          835    i.hal_dsi_tx_init_video_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017780   0x00017780   0x00000044   Code   RO          836    i.hal_dsi_tx_send_cmd  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000177c4   0x000177c4   0x00000028   Code   RO          909    i.hal_gpio_init_output  CVWL568.lib(hal_gpio.o)
    0x000177ec   0x000177ec   0x00000060   Code   RO          913    i.hal_gpio_set_mode  CVWL568.lib(hal_gpio.o)
    0x0001784c   0x0001784c   0x00000008   Code   RO          914    i.hal_gpio_set_output_data  CVWL568.lib(hal_gpio.o)
    0x00017854   0x00017854   0x00000018   Code   RO         1107    i.hal_internal_check_video_auto_sync  CVWL568.lib(hal_internal_vsync.o)
    0x0001786c   0x0001786c   0x000000fc   Code   RO         1108    i.hal_internal_init_memc  CVWL568.lib(hal_internal_vsync.o)
    0x00017968   0x00017968   0x0000002a   Code   RO         1109    i.hal_internal_rx_dcs_async_handler  CVWL568.lib(hal_internal_vsync.o)
    0x00017992   0x00017992   0x00000002   PAD
    0x00017994   0x00017994   0x00000058   Code   RO         1110    i.hal_internal_rx_dcs_polling  CVWL568.lib(hal_internal_vsync.o)
    0x000179ec   0x000179ec   0x00000010   Code   RO         1112    i.hal_internal_sync_get_fb_setting  CVWL568.lib(hal_internal_vsync.o)
    0x000179fc   0x000179fc   0x00000010   Code   RO         1113    i.hal_internal_sync_get_hight_performan_mode  CVWL568.lib(hal_internal_vsync.o)
    0x00017a0c   0x00017a0c   0x0000022c   Code   RO         1114    i.hal_internal_sync_input_resolution_change  CVWL568.lib(hal_internal_vsync.o)
    0x00017c38   0x00017c38   0x00000028   Code   RO         1117    i.hal_internal_vsync_deinit  CVWL568.lib(hal_internal_vsync.o)
    0x00017c60   0x00017c60   0x00000018   Code   RO         1119    i.hal_internal_vsync_get_sync_line  CVWL568.lib(hal_internal_vsync.o)
    0x00017c78   0x00017c78   0x0000000c   Code   RO         1120    i.hal_internal_vsync_get_tear_mode  CVWL568.lib(hal_internal_vsync.o)
    0x00017c84   0x00017c84   0x0000000c   Code   RO         1121    i.hal_internal_vsync_get_tx_state  CVWL568.lib(hal_internal_vsync.o)
    0x00017c90   0x00017c90   0x00000140   Code   RO         1122    i.hal_internal_vsync_init_rx  CVWL568.lib(hal_internal_vsync.o)
    0x00017dd0   0x00017dd0   0x000000b0   Code   RO         1123    i.hal_internal_vsync_init_tx  CVWL568.lib(hal_internal_vsync.o)
    0x00017e80   0x00017e80   0x00000090   Code   RO         1125    i.hal_internal_vsync_set_auto_hw_filter  CVWL568.lib(hal_internal_vsync.o)
    0x00017f10   0x00017f10   0x00000024   Code   RO         1127    i.hal_internal_vsync_set_rx_state  CVWL568.lib(hal_internal_vsync.o)
    0x00017f34   0x00017f34   0x00000044   Code   RO         1128    i.hal_internal_vsync_set_sync_line  CVWL568.lib(hal_internal_vsync.o)
    0x00017f78   0x00017f78   0x00000050   Code   RO         1129    i.hal_internal_vsync_set_tear_mode  CVWL568.lib(hal_internal_vsync.o)
    0x00017fc8   0x00017fc8   0x00000084   Code   RO         1130    i.hal_internal_vsync_set_tx_state  CVWL568.lib(hal_internal_vsync.o)
    0x0001804c   0x0001804c   0x00000010   Code   RO         1716    i.hal_intl_svs_deinit_tx  CVWL568.lib(hal_internal_soft_sync.o)
    0x0001805c   0x0001805c   0x00000024   Code   RO         1717    i.hal_intl_svs_handle  CVWL568.lib(hal_internal_soft_sync.o)
    0x00018080   0x00018080   0x00000078   Code   RO         1718    i.hal_intl_svs_init_rx  CVWL568.lib(hal_internal_soft_sync.o)
    0x000180f8   0x000180f8   0x00000014   Code   RO         1719    i.hal_intl_svs_init_tx  CVWL568.lib(hal_internal_soft_sync.o)
    0x0001810c   0x0001810c   0x0000000c   Code   RO         1721    i.hal_intl_svs_set_sync_coef  CVWL568.lib(hal_internal_soft_sync.o)
    0x00018118   0x00018118   0x00000048   Code   RO         1722    i.hal_intl_svs_update_rxbr_clk  CVWL568.lib(hal_internal_soft_sync.o)
    0x00018160   0x00018160   0x00000024   Code   RO          837    i.hal_lcdc_config_ccm  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018184   0x00018184   0x00000064   Code   RO          838    i.hal_lcdc_config_remains  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000181e8   0x000181e8   0x00000014   Code   RO          839    i.hal_lcdc_config_rgb_to_pentile  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000181fc   0x000181fc   0x00000164   Code   RO          840    i.hal_lcdc_config_upscaler  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018360   0x00018360   0x00000054   Code   RO          841    i.hal_lcdc_init_cfg  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000183b4   0x000183b4   0x000001cc   Code   RO          842    i.hal_lcdc_init_clk  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018580   0x00018580   0x00000040   Code   RO          843    i.hal_lcdc_init_interrupt  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000185c0   0x000185c0   0x00000008   Code   RO         1028    i.hal_system_enable_systick  CVWL568.lib(hal_system.o)
    0x000185c8   0x000185c8   0x00000088   Code   RO         1032    i.hal_system_init   CVWL568.lib(hal_system.o)
    0x00018650   0x00018650   0x0000001c   Code   RO         1033    i.hal_system_init_console  CVWL568.lib(hal_system.o)
    0x0001866c   0x0001866c   0x00000008   Code   RO         1036    i.hal_system_set_phy_calibration  CVWL568.lib(hal_system.o)
    0x00018674   0x00018674   0x00000030   Code   RO          844    i.hal_tx_frame_rate_adjust  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000186a4   0x000186a4   0x0000008c   Code   RO         1082    i.hal_uart_init     CVWL568.lib(hal_uart.o)
    0x00018730   0x00018730   0x00000010   Code   RO         1085    i.hal_uart_transmit_blocking  CVWL568.lib(hal_uart.o)
    0x00018740   0x00018740   0x00000110   Code   RO         2216    i.handle_init       CVWL568.lib(irq_redirect .o)
    0x00018850   0x00018850   0x0000006c   Code   RO          115    i.init_mipi_tx      ap_demo.o
    0x000188bc   0x000188bc   0x000000a0   Code   RO          116    i.init_panel        ap_demo.o
    0x0001895c   0x0001895c   0x0000000a   Code   RO            3    i.main              main.o
    0x00018966   0x00018966   0x00000002   PAD
    0x00018968   0x00018968   0x000000d4   Code   RO          117    i.open_mipi_rx      ap_demo.o
    0x00018a3c   0x00018a3c   0x0000009c   Code   RO          118    i.pps_update_handle  ap_demo.o
    0x00018ad8   0x00018ad8   0x000003f4   Code   RO         1134    i.rx_get_dcs_packet_data  CVWL568.lib(hal_internal_vsync.o)
    0x00018ecc   0x00018ecc   0x0000016c   Code   RO         1135    i.rx_partial_update  CVWL568.lib(hal_internal_vsync.o)
    0x00019038   0x00019038   0x0000008c   Code   RO         1136    i.rx_receive_packet  CVWL568.lib(hal_internal_vsync.o)
    0x000190c4   0x000190c4   0x00000180   Code   RO         1137    i.rx_receive_pps    CVWL568.lib(hal_internal_vsync.o)
    0x00019244   0x00019244   0x000000cc   Code   RO         1138    i.rxbr_irq0_callback  CVWL568.lib(hal_internal_vsync.o)
    0x00019310   0x00019310   0x00000244   Code   RO         1139    i.rxbr_irq1_callback  CVWL568.lib(hal_internal_vsync.o)
    0x00019554   0x00019554   0x000000c4   Code   RO         1140    i.soft_gen_te       CVWL568.lib(hal_internal_vsync.o)
    0x00019618   0x00019618   0x000000c0   Code   RO         1141    i.soft_gen_te_double_buffer  CVWL568.lib(hal_internal_vsync.o)
    0x000196d8   0x000196d8   0x00000048   Code   RO         2733    i.sqrt              m_ps.l(sqrt.o)
    0x00019720   0x00019720   0x000000ac   Code   RO         1723    i.svs_direct_mode_setting  CVWL568.lib(hal_internal_soft_sync.o)
    0x000197cc   0x000197cc   0x0000001c   Code   RO         1724    i.svs_get_rel_intv  CVWL568.lib(hal_internal_soft_sync.o)
    0x000197e8   0x000197e8   0x000000b0   Code   RO         1725    i.svs_sync_handle   CVWL568.lib(hal_internal_soft_sync.o)
    0x00019898   0x00019898   0x000000f4   Code   RO         1726    i.svs_wait_start    CVWL568.lib(hal_internal_soft_sync.o)
    0x0001998c   0x0001998c   0x000000d8   Code   RO         1727    i.svs_waite_fr_stab  CVWL568.lib(hal_internal_soft_sync.o)
    0x00019a64   0x00019a64   0x00000108   Code   RO         1142    i.vidc_callback     CVWL568.lib(hal_internal_vsync.o)
    0x00019b6c   0x00019b6c   0x000000d8   Code   RO         1143    i.vpre_err_reset    CVWL568.lib(hal_internal_vsync.o)
    0x00019c44   0x00019c44   0x000001cc   Code   RO         1144    i.vsync_set_te_mode  CVWL568.lib(hal_internal_vsync.o)
    0x00019e10   0x00019e10   0x00001f74   Data   RO          122    .constdata          ap_demo.o
    0x0001bd84   0x0001bd84   0x000000d2   Data   RO          919    .constdata          CVWL568.lib(hal_gpio.o)
    0x0001be56   0x0001be56   0x00000002   PAD
    0x0001be58   0x0001be58   0x00000008   Data   RO         1597    .constdata          CVWL568.lib(drv_param_init.o)
    0x0001be60   0x0001be60   0x00000186   Data   RO         2288    .constdata          CVWL568.lib(drv_phy_common.o)
    0x0001bfe6   0x0001bfe6   0x00000002   PAD
    0x0001bfe8   0x0001bfe8   0x00000048   Data   RO          744    .conststring        CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001c030   0x0001c030   0x00000043   Data   RO          847    .conststring        CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001c073   0x0001c073   0x00000001   PAD
    0x0001c074   0x0001c074   0x00000178   Data   RO         1146    .conststring        CVWL568.lib(hal_internal_vsync.o)
    0x0001c1ec   0x0001c1ec   0x00000030   Data   RO         3097    Region$$Table       anon$$obj.o


    Execution Region RW_RAM1 (Exec base: 0x00070000, Load base: 0x0001c21c, Size: 0x00000000, Max: 0x000000f0, ABSOLUTE)

    **** No section assigned to this execution region ****


    Execution Region RW_RAM2 (Exec base: 0x00070100, Load base: 0x0001c21c, Size: 0x000000c0, Max: 0x000000d0, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00070100        -       0x000000c0   Zero   RW         2217    .ARM.__AT_0x00070100  CVWL568.lib(irq_redirect .o)


    Execution Region RW_RAM3 (Exec base: 0x000701d0, Load base: 0x0001c21c, Size: 0x00003650, Max: 0x00007e30, ABSOLUTE, COMPRESSED[0x0000052c])

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x000701d0   COMPRESSED   0x00000230   Data   RW          123    .data               ap_demo.o
    0x00070400   COMPRESSED   0x0000003b   Data   RW          436    .data               app_tp_st_touch.o
    0x0007043b   COMPRESSED   0x00000001   PAD
    0x0007043c   COMPRESSED   0x000000e4   Data   RW          588    .data               WL568_S21_NT37701_TP.lib(app_tp_for_custom_s8.o)
    0x00070520   COMPRESSED   0x00000008   Data   RW          745    .data               CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00070528   COMPRESSED   0x00000003   Data   RW          848    .data               CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0007052b   COMPRESSED   0x00000001   PAD
    0x0007052c   COMPRESSED   0x00000018   Data   RW         1147    .data               CVWL568.lib(hal_internal_vsync.o)
    0x00070544   COMPRESSED   0x0000000c   Data   RW         1208    .data               CVWL568.lib(drv_common.o)
    0x00070550   COMPRESSED   0x00000004   Data   RW         1475    .data               CVWL568.lib(drv_gpio.o)
    0x00070554   COMPRESSED   0x00000004   Data   RW         1542    .data               CVWL568.lib(drv_i2c_master.o)
    0x00070558   COMPRESSED   0x00000004   Data   RW         1573    .data               CVWL568.lib(drv_i2c_slave.o)
    0x0007055c   COMPRESSED   0x000004a4   Data   RW         1598    .data               CVWL568.lib(drv_param_init.o)
    0x00070a00   COMPRESSED   0x00000004   Data   RW         1665    .data               CVWL568.lib(drv_spi_master.o)
    0x00070a04   COMPRESSED   0x00000001   Data   RW         1697    .data               CVWL568.lib(drv_sys_cfg.o)
    0x00070a05   COMPRESSED   0x00000003   PAD
    0x00070a08   COMPRESSED   0x00000008   Data   RW         2066    .data               CVWL568.lib(drv_rxbr.o)
    0x00070a10   COMPRESSED   0x00000004   Data   RW         2142    .data               CVWL568.lib(drv_vidc.o)
    0x00070a14   COMPRESSED   0x00000001   Data   RW         2289    .data               CVWL568.lib(drv_phy_common.o)
    0x00070a15   COMPRESSED   0x00000003   PAD
    0x00070a18   COMPRESSED   0x0000000c   Data   RW         2309    .data               CVWL568.lib(drv_chip_info.o)
    0x00070a24   COMPRESSED   0x00000012   Data   RW         2418    .data               CVWL568.lib(norflash.o)
    0x00070a36   COMPRESSED   0x00000002   PAD
    0x00070a38   COMPRESSED   0x0000000c   Data   RW         2505    .data               CVWL568.lib(drv_pwm.o)
    0x00070a44   COMPRESSED   0x00000008   Data   RW         2560    .data               CVWL568.lib(drv_swire.o)
    0x00070a4c   COMPRESSED   0x00000050   Data   RW         2587    .data               CVWL568.lib(drv_timer.o)
    0x00070a9c   COMPRESSED   0x00000008   Data   RW         2637    .data               CVWL568.lib(drv_uart.o)
    0x00070aa4   COMPRESSED   0x0000000c   Data   RW         2704    .data               CVWL568.lib(drv_wdg.o)
    0x00070ab0   COMPRESSED   0x00000004   Data   RW         3066    .data               mc_p.l(stdout.o)
    0x00070ab4   COMPRESSED   0x00000004   Data   RW         3078    .data               mc_p.l(errno.o)
    0x00070ab8        -       0x00000024   Zero   RW          121    .bss                ap_demo.o
    0x00070adc        -       0x000000c4   Zero   RW          743    .bss                CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00070ba0        -       0x0000004c   Zero   RW          845    .bss                CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00070bec        -       0x00000100   Zero   RW         1072    .bss                CVWL568.lib(tau_log.o)
    0x00070cec        -       0x000000d0   Zero   RW         1087    .bss                CVWL568.lib(hal_uart.o)
    0x00070dbc        -       0x00000974   Zero   RW         1145    .bss                CVWL568.lib(hal_internal_vsync.o)
    0x00071730        -       0x0000001c   Zero   RW         1337    .bss                CVWL568.lib(drv_dma.o)
    0x0007174c        -       0x00000040   Zero   RW         1474    .bss                CVWL568.lib(drv_gpio.o)
    0x0007178c        -       0x00000040   Zero   RW         1728    .bss                CVWL568.lib(hal_internal_soft_sync.o)
    0x000717cc        -       0x00000020   Zero   RW         2353    .bss                CVWL568.lib(hal_spi_slave.o)
    0x000717ec        -       0x00001030   Zero   RW         2722    .bss                CVWL568.lib(dcs_packet_fifo.o)
    0x0007281c   COMPRESSED   0x00000004   PAD
    0x00072820        -       0x00001000   Zero   RW          560    STACK               startup_armcm0.o


==============================================================================

Image component sizes


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Object Name

      5942        656       8052        560         36      28371   ap_demo.o
        32          4          0         59          0       4580   app_tp_st_touch.o
        36          6          0          0          0        565   board.o
        10          0          0          0          0       5715   main.o
       120         18        192          0       4096       2124   startup_armcm0.o

    ----------------------------------------------------------------------
      6144        684       8292        620       4132      41355   Object Totals
         0          0         48          0          0          0   (incl. Generated)
         4          0          0          1          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Member Name

       216         32          0          0       4144        252   dcs_packet_fifo.o
       272         96          0         12          0        256   drv_chip_info.o
       192         82         24         12          0        264   drv_common.o
       420         90          0          0          0       1200   drv_crgu.o
       196         12          0          0         28        272   drv_dma.o
       232         28          0          0          0        340   drv_dsc_dec.o
      1658        494          0          0          0       1396   drv_dsi_rx.o
      1528        118          0          0          0       2428   drv_dsi_tx.o
       132          0          0          0          0        256   drv_efuse.o
        10          0          0          0          0         60   drv_fls.o
       356         74          0          4         64        912   drv_gpio.o
        16          8          0          4          0         60   drv_i2c_master.o
        24         10          0          4          0         60   drv_i2c_slave.o
       704          6          0          0          0       1504   drv_lcdc.o
       492         28          0          0          0       1112   drv_memc.o
       212         44          8       1188          0        452   drv_param_init.o
       428         30        390          1          0        664   drv_phy_common.o
        72         10          0         12          0         76   drv_pwm.o
        80         18          0          0          0        120   drv_pwr.o
       560         74          0          8          0       1560   drv_rxbr.o
        72         20          0          4          0        128   drv_spi_master.o
       116         12          0          8          0        140   drv_swire.o
       168         34          0          1          0        320   drv_sys_cfg.o
       282         16          0         80          0        680   drv_timer.o
       698         18          0          8          0        680   drv_uart.o
       510         28          0          4          0       1452   drv_vidc.o
       168         22          0         12          0        316   drv_wdg.o
      3090        294         72          8        196       1620   hal_dsi_rx_ctrl.o
      4256        288         67          3         76       2336   hal_dsi_tx_ctrl.o
       176         18        210          0          0        264   hal_gpio.o
      1112        188          0          0         64        776   hal_internal_soft_sync.o
      8052       1622        376         24       2420       2680   hal_internal_vsync.o
       580         32          0          0         32        136   hal_spi_slave.o
       180         32          0          0          0        272   hal_system.o
       156         18          0          0        208        144   hal_uart.o
      1076        324          0          0        192       1980   irq_redirect .o
        48         10          0         18          0         68   norflash.o
        58          0          0          0          0        128   tau_delay.o
        60         10          0          0        256        156   tau_log.o
         0          0          0        228          0      15807   app_tp_for_custom_s8.o
       200         20          0          0          0         76   ceil.o
        72          6          0          0          0         76   sqrt.o
        86          0          0          0          0          0   __dczerorl2.o
         0          0          0          0          0          0   entry.o
         0          0          0          0          0          0   entry10a.o
         0          0          0          0          0          0   entry11a.o
         8          4          0          0          0          0   entry2.o
         4          0          0          0          0          0   entry5.o
         0          0          0          0          0          0   entry7b.o
         0          0          0          0          0          0   entry8b.o
         8          4          0          0          0          0   entry9a.o
        12          6          0          4          0         60   errno.o
        30          0          0          0          0          0   handlers.o
        40          0          0          0          0         72   idiv.o
        36          8          0          0          0         68   init.o
         0          0          0          0          0          0   iusefp.o
        32          0          0          0          0         68   llshl.o
        38          0          0          0          0         68   llsshr.o
        34          0          0          0          0         68   llushr.o
        36          0          0          0          0         60   memcpya.o
        36          0          0          0          0        100   memseta.o
      2298        104          0          0          0        544   printfa.o
         0          0          0          4          0          0   stdout.o
        44          0          0          0          0         72   uidiv.o
        96          0          0          0          0         84   uldiv.o
        40          2          0          0          0         68   cdcmple.o
        40          2          0          0          0         68   cdrcmple.o
        20          0          0          0          0         68   cfcmple.o
        20          0          0          0          0         68   cfrcmple.o
       356          4          0          0          0        140   dadd.o
       240          6          0          0          0         84   ddiv.o
       236          0          0          0          0        216   depilogue.o
        72         10          0          0          0         72   dfixi.o
        60         10          0          0          0         68   dfixui.o
        64         10          0          0          0         68   dfixul.o
        28          4          0          0          0         68   dfltui.o
       208          6          0          0          0         88   dmul.o
       162          0          0          0          0         80   dsqrt.o
        40          0          0          0          0         60   f2d.o
       178          0          0          0          0        108   fadd.o
       124          0          0          0          0         72   fdiv.o
       130          0          0          0          0        144   fepilogue.o
        50          0          0          0          0         60   ffixi.o
        40          0          0          0          0         60   ffixui.o
        22          0          0          0          0         68   fflti.o
        14          0          0          0          0         68   ffltui.o
       122          0          0          0          0         72   fmul.o
        24          0          0          0          0         60   fscalb.o

    ----------------------------------------------------------------------
     34104       4446       1152       1660       7684      46671   Library Totals
        46          0          5          9          4          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Name

     28658       4240       1147       1415       7680      27520   CVWL568.lib
         0          0          0        228          0      15807   WL568_S21_NT37701_TP.lib
       272         26          0          0          0        152   m_ps.l
      2838        126          0          8          0       1264   mc_p.l
      2290         54          0          0          0       1928   mf_p.l

    ----------------------------------------------------------------------
     34104       4446       1152       1660       7684      46671   Library Totals

    ----------------------------------------------------------------------

==============================================================================


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   

     40248       5130       9444       2280      11816      67494   Grand Totals
     40248       5130       9444       1324      11816      67494   ELF Image Totals (compressed)
     40248       5130       9444       1324          0          0   ROM Totals

==============================================================================

    Total RO  Size (Code + RO Data)                49692 (  48.53kB)
    Total RW  Size (RW Data + ZI Data)             14096 (  13.77kB)
    Total ROM Size (Code + RO Data + RW Data)      51016 (  49.82kB)

==============================================================================

