Component: ARM Compiler 5.06 update 6 (build 750) Tool: armlink [4d35ed]

==============================================================================

Section Cross References

    main.o(i.main) refers to board.o(i.board_Init) for board_Init
    main.o(i.main) refers to ap_demo.o(i.ap_demo) for ap_demo
    ap_demo.o(i.Gpio_swire_output) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    ap_demo.o(i.Gpio_swire_output) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.Gpio_swire_output) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    ap_demo.o(i.Gpio_swire_output) refers to tau_delay.o(i.delayUs) for delayUs
    ap_demo.o(i.PhoneDisOffDeal) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    ap_demo.o(i.PhoneDisOffDeal) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    ap_demo.o(i.PhoneDisOffDeal) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    ap_demo.o(i.PhoneDisOffDeal) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.PhoneDisOffDeal) refers to hal_system.o(i.hal_system_get_tick) for hal_system_get_tick
    ap_demo.o(i.PhoneDisOffDeal) refers to printfa.o(i.__0printf) for __2printf
    ap_demo.o(i.PhoneDisOffDeal) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) for hal_dsi_rx_ctrl_get_max_ret_size
    ap_demo.o(i.ap_dcs_read) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) for hal_dsi_rx_ctrl_send_ack_cmd
    ap_demo.o(i.ap_dcs_read) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_dcs_read) refers to app_tp_st_touch.o(i.ap_get_tp_calibration_status_01) for ap_get_tp_calibration_status_01
    ap_demo.o(i.ap_demo) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.open_mipi_rx) for open_mipi_rx
    ap_demo.o(i.ap_demo) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.init_mipi_tx) for init_mipi_tx
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.init_panel) for init_panel
    ap_demo.o(i.ap_demo) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    ap_demo.o(i.ap_demo) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.ap_demo) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_demo) refers to ap_demo.o(i.PhoneDisOffDeal) for PhoneDisOffDeal
    ap_demo.o(i.ap_demo) refers to memcpya.o(.text) for __aeabi_memcpy4
    ap_demo.o(i.ap_demo) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) for hal_dsi_tx_ctrl_set_ccm
    ap_demo.o(i.ap_demo) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) for hal_dsi_rx_ctrl_dsc_async_handler
    ap_demo.o(i.ap_demo) refers to app_tp_for_custom_s8.o(.data) for tp_sleep_in
    ap_demo.o(i.ap_demo) refers to ap_demo.o(.bss) for .bss
    ap_demo.o(i.ap_demo) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_get_reg_df) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_get_reg_df) refers to ap_demo.o(.bss) for .bss
    ap_demo.o(i.ap_set_backlight_51) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_backlight_51) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_backlight_51) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_set_display_off) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_display_off) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_display_on) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to ap_demo.o(i.Gpio_swire_output) for Gpio_swire_output
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin) for hal_dsi_tx_ctrl_panel_reset_pin
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_enter_sleep_mode) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_set_exit_sleep_mode) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.ap_set_exit_sleep_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_exit_sleep_mode) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.ap_set_exit_sleep_mode) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) for hal_dsi_rx_ctrl_toggle_resolution
    ap_demo.o(i.ap_set_exit_sleep_mode) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_set_hbm_53) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.ap_set_hbm_53) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.ap_update_frame_rate) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex) for hal_dsi_rx_ctrl_set_tear_mode_ex
    ap_demo.o(i.ap_update_frame_rate) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.frame_start_cb) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) for hal_dsi_rx_ctrl_restart
    ap_demo.o(i.frame_start_cb) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.frame_start_cb) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.init_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) for hal_dsi_tx_ctrl_create_handle
    ap_demo.o(i.init_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    ap_demo.o(i.init_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) for hal_dsi_tx_ctrl_set_overwrite_rgb
    ap_demo.o(i.init_mipi_tx) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin) for hal_dsi_tx_ctrl_panel_reset_pin
    ap_demo.o(i.init_panel) refers to tau_delay.o(i.delayMs) for delayMs
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) for hal_dsi_tx_ctrl_enter_init_panel_mode
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) for hal_dsi_tx_ctrl_write_array_cmd
    ap_demo.o(i.init_panel) refers to tau_delay.o(i.delayUs) for delayUs
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    ap_demo.o(i.init_panel) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    ap_demo.o(i.init_panel) refers to ap_demo.o(i.Gpio_swire_output) for Gpio_swire_output
    ap_demo.o(i.init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) for hal_dsi_tx_ctrl_exit_init_panel_mode
    ap_demo.o(i.init_panel) refers to ap_demo.o(.constdata) for .constdata
    ap_demo.o(i.open_mipi_rx) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) for hal_dsi_rx_ctrl_create_handle
    ap_demo.o(i.open_mipi_rx) refers to memcpya.o(.text) for __aeabi_memcpy4
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) for hal_dsi_rx_ctrl_pre_init_pps
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) for hal_dsi_rx_ctrl_set_cus_sync_line
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) for hal_dsi_rx_ctrl_set_cus_scld_filter
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    ap_demo.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) for hal_dsi_rx_ctrl_set_cus_esc_clk
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(.constdata) for .constdata
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(i.ap_dcs_read) for ap_dcs_read
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(i.pps_update_handle) for pps_update_handle
    ap_demo.o(i.open_mipi_rx) refers to ap_demo.o(i.frame_start_cb) for frame_start_cb
    ap_demo.o(i.pps_update_handle) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) for hal_dsi_rx_ctrl_toggle_resolution
    ap_demo.o(i.pps_update_handle) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.pps_update_handle) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.tp_heartbeat_exec) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    ap_demo.o(i.tp_heartbeat_exec) refers to tau_log.o(i.LOG_printf) for LOG_printf
    ap_demo.o(i.tp_heartbeat_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) for ap_tp_st_touch_hardware_reset
    ap_demo.o(i.tp_heartbeat_exec) refers to app_tp_transfer.o(.data) for s_screen_init_complate
    ap_demo.o(i.tp_heartbeat_exec) refers to ap_demo.o(.data) for .data
    ap_demo.o(i.tp_power_up_restart) refers to app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) for ap_tp_st_touch_hardware_reset
    ap_demo.o(i.tp_power_up_restart) refers to ap_demo.o(.data) for .data
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_display_on) for ap_set_display_on
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_display_off) for ap_set_display_off
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_get_reg_df) for ap_get_reg_df
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_backlight_51) for ap_set_backlight_51
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_update_frame_rate) for ap_update_frame_rate
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_hbm_53) for ap_set_hbm_53
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_enter_sleep_mode) for ap_set_enter_sleep_mode
    ap_demo.o(.constdata) refers to ap_demo.o(i.ap_set_exit_sleep_mode) for ap_set_exit_sleep_mode
    app_tp_transfer.o(i.S20_Start_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_transfer.o(i.S20_Start_init) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.S20_Start_init) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_ctrl_eint) for hal_gpio_ctrl_eint
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_init_eint) for hal_gpio_init_eint
    app_tp_transfer.o(i.S20_Start_init) refers to hal_gpio.o(i.hal_gpio_reg_eint_cb) for hal_gpio_reg_eint_cb
    app_tp_transfer.o(i.S20_Start_init) refers to ap_demo.o(.data) for s_power_up_flag
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_for_custom_s8.o(.data) for screen_reg_int_data
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.S20_Start_init) refers to app_tp_transfer.o(i.app_tp_screen_int_callback) for app_tp_screen_int_callback
    app_tp_transfer.o(i.S20_Start_init) refers to ap_demo.o(.data) for phone_start_flag
    app_tp_transfer.o(i.app_tp_I2C_init) refers to hal_i2c_slave.o(i.hal_i2c_s_init) for hal_i2c_s_init
    app_tp_transfer.o(i.app_tp_I2C_init) refers to hal_i2c_slave.o(i.hal_i2c_s_set_transfer) for hal_i2c_s_set_transfer
    app_tp_transfer.o(i.app_tp_I2C_init) refers to hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read) for hal_i2c_s_nonblocking_read
    app_tp_transfer.o(i.app_tp_I2C_init) refers to app_tp_transfer.o(i.app_tp_i2cs_callback) for app_tp_i2cs_callback
    app_tp_transfer.o(i.app_tp_I2C_init) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_st_touch.o(i.app_tp_phone_analysis_data_for_wake_up) for app_tp_phone_analysis_data_for_wake_up
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) for app_tp_phone_analysis_data
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(i.app_tp_s_read) for app_tp_s_read
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(i.app_tp_s_write) for app_tp_s_write
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_st_touch.o(.data) for g_tp_wakeup_response
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.app_tp_init) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    app_tp_transfer.o(i.app_tp_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    app_tp_transfer.o(i.app_tp_init) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_master.o(i.hal_i2c_m_dma_init) for hal_i2c_m_dma_init
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_for_custom_s8.o(.data) for g_phone_output_int_pad
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.app_tp_m_read) refers to hal_i2c_master.o(i.hal_i2c_m_dma_read) for hal_i2c_m_dma_read
    app_tp_transfer.o(i.app_tp_m_transfer_complate) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.app_tp_m_write) refers to hal_i2c_master.o(i.hal_i2c_m_dma_write) for hal_i2c_m_dma_write
    app_tp_transfer.o(i.app_tp_phone_clear_reset_on) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_phone_reset_on) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_s_read) refers to hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read) for hal_i2c_s_nonblocking_read
    app_tp_transfer.o(i.app_tp_s_transfer_complate) refers to hal_i2c_slave.o(i.hal_i2c_s_write_complate) for hal_i2c_s_write_complate
    app_tp_transfer.o(i.app_tp_s_transfer_complate) refers to hal_i2c_slave.o(i.hal_i2c_s_read_complate) for hal_i2c_s_read_complate
    app_tp_transfer.o(i.app_tp_s_write) refers to hal_i2c_slave.o(i.hal_i2c_s_dma_write) for hal_i2c_s_dma_write
    app_tp_transfer.o(i.app_tp_screen_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    app_tp_transfer.o(i.app_tp_screen_init) refers to tau_delay.o(i.delayUs) for delayUs
    app_tp_transfer.o(i.app_tp_screen_init) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_transfer.o(i.app_tp_screen_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_rst_pad
    app_tp_transfer.o(i.app_tp_screen_int_callback) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to hal_spi_master.o(i.hal_spi_m_clear_rxfifo) for hal_spi_m_clear_rxfifo
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(i.S20_Start_init) for S20_Start_init
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_for_custom_s8.o(.constdata) for screen_reg_start_data_size
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to ap_demo.o(.data) for phone_start_flag
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_st_touch.o(i.app_tp_screen_analysis_wake_up_exec) for app_tp_screen_analysis_wake_up_exec
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_transfer_screen_const) for app_tp_transfer_screen_const
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_F3) for ap_tp_st_touch_error_handler_F3
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_FF) for ap_tp_st_touch_error_handler_FF
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event) for ap_tp_st_touch_scan_point_record_event
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_st_touch.o(i.app_tp_screen_analysis_wake_up) for app_tp_screen_analysis_wake_up
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) for app_tp_screen_analysis_int
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to tau_delay.o(i.delayUs) for delayUs
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(.data) for .data
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(.data) for screen_reg_int_data
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(.bss) for .bss
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(.data) for tp_sleep_in
    app_tp_transfer.o(i.app_tp_transfer_screen_start) refers to app_tp_transfer.o(i.app_tp_transfer_screen_const) for app_tp_transfer_screen_const
    app_tp_transfer.o(i.app_tp_transfer_screen_start) refers to app_tp_transfer.o(.data) for .data
    app_tp_st_touch.o(i.CRC16_2) refers to app_tp_st_touch.o(.constdata) for .constdata
    app_tp_st_touch.o(i.ap_get_tp_calibration_status_01) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) for hal_dsi_rx_ctrl_send_ack_cmd
    app_tp_st_touch.o(i.ap_get_tp_calibration_status_01) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.ap_set_tp_calibration_04) refers to memseta.o(.text) for __aeabi_memclr4
    app_tp_st_touch.o(i.ap_set_tp_calibration_04) refers to printfa.o(i.__0printf) for __2printf
    app_tp_st_touch.o(i.ap_set_tp_calibration_04) refers to app_tp_st_touch.o(i.CRC16_2) for CRC16_2
    app_tp_st_touch.o(i.ap_set_tp_calibration_04) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.ap_tp_st_touch_calibration) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_st_touch.o(i.ap_tp_st_touch_calibration) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_st_touch.o(i.ap_tp_st_touch_calibration) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_calibration) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_F3) refers to app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) for ap_tp_st_touch_software_reset
    app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_FF) refers to app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) for ap_tp_st_touch_software_reset
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to memseta.o(.text) for __aeabi_memclr4
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to tau_log.o(i.LOG_printf) for LOG_printf
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_rst_pad
    app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init) refers to app_tp_st_touch.o(.bss) for .bss
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event) refers to app_tp_st_touch.o(.bss) for .bss
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec) refers to printfa.o(i.__0printf) for __2printf
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event) for ap_tp_st_touch_simulate_finger_release_event
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init) for ap_tp_st_touch_scan_point_init
    app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec) refers to app_tp_st_touch.o(.bss) for .bss
    app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event) refers to app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) for app_tp_screen_analysis_int
    app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event) for ap_tp_st_touch_simulate_finger_release_event
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init) for ap_tp_st_touch_scan_point_init
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to hal_i2c_master.o(i.hal_i2c_m_transfer_complate) for hal_i2c_m_transfer_complate
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.ap_tp_st_touch_software_reset) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_calibration) for ap_tp_st_touch_calibration
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark) for ap_tp_st_touch_get_calibration_success_mark
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to tau_log.o(i.LOG_printf) for LOG_printf
    app_tp_st_touch.o(i.app_tp_calibration_exec) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.app_tp_phone_analysis_data_for_wake_up) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_st_touch.o(i.app_tp_phone_analysis_data_for_wake_up) refers to app_tp_for_custom_s8.o(.data) for g_phone_output_int_pad
    app_tp_st_touch.o(i.app_tp_phone_analysis_data_for_wake_up) refers to app_tp_st_touch.o(.bss) for .bss
    app_tp_st_touch.o(i.app_tp_phone_analysis_data_for_wake_up) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.app_tp_screen_analysis_wake_up) refers to app_tp_st_touch.o(.bss) for .bss
    app_tp_st_touch.o(i.app_tp_screen_analysis_wake_up) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.app_tp_screen_analysis_wake_up_exec) refers to tau_log.o(i.LOG_printf) for LOG_printf
    app_tp_st_touch.o(i.app_tp_screen_analysis_wake_up_exec) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_st_touch.o(i.app_tp_screen_analysis_wake_up_exec) refers to app_tp_st_touch.o(.data) for .data
    app_tp_st_touch.o(i.app_tp_screen_analysis_wake_up_exec) refers to app_tp_st_touch.o(.bss) for .bss
    app_tp_st_touch.o(i.app_tp_screen_analysis_wake_up_exec) refers to app_tp_for_custom_s8.o(.data) for g_phone_output_int_pad
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_init) for hal_system_init
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_enable_systick) for hal_system_enable_systick
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_init_console) for hal_system_init_console
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_set_phy_calibration) for hal_system_set_phy_calibration
    startup_armcm0.o(RESET) refers to startup_armcm0.o(STACK) for __initial_sp
    startup_armcm0.o(RESET) refers to startup_armcm0.o(.text) for Reset_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.HardFault_Handler) for HardFault_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SysTick_Handler) for SysTick_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.VIDC_IRQn_Handler) for VIDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.LCDC_IRQn_Handler) for LCDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.MIPI_RX_IRQn_Handler) for MIPI_RX_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.MIPI_TX_IRQn_Handler) for MIPI_TX_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.MEMC_IRQn_Handler) for MEMC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.VPRE_IRQn_Handler) for VPRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.FLSCTRL_IRQn_Handler) for FLSCTRL_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.DMA_IRQn_Handler) for DMA_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER0_IRQn_Handler) for TIMER0_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER1_IRQn_Handler) for TIMER1_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER2_IRQn_Handler) for TIMER2_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.TIMER3_IRQn_Handler) for TIMER3_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.WDG_IRQn_Handler) for WDG_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.UART_IRQn_Handler) for UART_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.I2C0_IRQn_Handler) for I2C0_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.I2C1_IRQn_Handler) for I2C1_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SPIS_IRQn_Handler) for SPIS_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SPIM_IRQn_Handler) for SPIM_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.ADC_IRQn_Handler) for ADC_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.PWMDET_IRQn_Handler) for PWMDET_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.SWIRE_IRQn_Handler) for SWIRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.AP_NRESET_IRQn_Handler) for AP_NRESET_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT0_IRQn_Handler) for EXTI_INT0_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT1_IRQn_Handler) for EXTI_INT1_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT2_IRQn_Handler) for EXTI_INT2_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT3_IRQn_Handler) for EXTI_INT3_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT4_IRQn_Handler) for EXTI_INT4_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT5_IRQn_Handler) for EXTI_INT5_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT6_IRQn_Handler) for EXTI_INT6_IRQn_Handler
    startup_armcm0.o(RESET) refers to irq_redirect .o(i.EXTI_INT7_IRQn_Handler) for EXTI_INT7_IRQn_Handler
    startup_armcm0.o(.text) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to app_tp_for_custom_s8.o(.data) for .data
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to app_tp_for_custom_s8.o(.constdata) for .constdata
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to app_tp_transfer.o(i.app_tp_screen_init) for app_tp_screen_init
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to app_tp_for_custom_s8.o(.data) for .data
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to uidiv.o(.text) for __aeabi_uidivmod
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to app_tp_for_custom_s8.o(.data) for .data
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_1
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_2
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_3
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_4
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_5
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_6
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for screen_data_write_7
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_point_data
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_point_back
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_coord_data
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.data) for phone_reg_coord_back
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video) refers to drv_vidc.o(i.drv_vidc_set_module_enable) for drv_vidc_set_module_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) for hal_internal_vsync_get_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to hal_internal_vsync.o(i.hal_internal_rx_dcs_async_handler) for hal_internal_rx_dcs_async_handler
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to hal_internal_vsync.o(i.hal_internal_rx_dcs_polling) for hal_internal_rx_dcs_polling
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg) for drv_dsi_rx_set_ddi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_crgu.o(i.drv_crgu_set_rxbr_src) for drv_crgu_set_rxbr_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_crgu.o(i.drv_crgu_set_rxbr_div) for drv_crgu_set_rxbr_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg) for drv_dsi_rx_set_ipi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_gen_a_tear_signal) for drv_memc_gen_a_tear_signal
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size) for drv_dsi_rx_get_max_ret_size
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) for hal_dsi_rx_ctrl_init_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_rx) for hal_internal_vsync_init_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) for hal_dsi_rx_ctrl_init_dsi_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) for hal_dsi_rx_ctrl_init_rxbr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps) for drv_dsc_dec_set_u8_pps
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) for hal_dsi_rx_ctrl_init_vidc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) for hal_dsi_rx_ctrl_init_memc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_chip_info.o(i.drv_chip_rx_init_done) for drv_chip_rx_init_done
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_vidc_src) for drv_crgu_set_vidc_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_fb_src) for drv_crgu_set_fb_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_fb_div) for drv_crgu_set_fb_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) for hal_dsi_rx_ctrl_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg) for drv_dsi_rx_set_ctrl_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) for drv_dsi_rx_set_up_phy
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap) for drv_dsi_rx_set_lane_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_inten) for drv_dsi_rx_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt) for drv_dsi_rx_set_resp_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_mode) for drv_memc_set_ltpo_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tear_mode) for hal_internal_vsync_get_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_vsync.o(i.hal_internal_check_video_auto_sync) for hal_internal_check_video_auto_sync
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_fs_en_conditions) for drv_memc_set_fs_en_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_lcdc_st_conditions) for drv_memc_set_lcdc_st_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_vidc_sync_cnt) for drv_memc_set_vidc_sync_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_double_buffer) for drv_memc_set_double_buffer
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_active_height) for drv_memc_set_active_height
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_inten) for drv_memc_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_color_format) for drv_rxbr_set_color_format
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th) for drv_rxbr_set_ltpo_drop_th
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_cfg) for drv_rxbr_set_usr_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_col) for drv_rxbr_set_usr_col
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_row) for drv_rxbr_set_usr_row
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg) for drv_rxbr_hline_rcv_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) for hal_internal_vsync_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_src_parameter) for drv_vidc_set_src_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pentile_swap) for drv_vidc_set_pentile_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_dst_parameter) for drv_vidc_set_dst_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_init_module_enable) for drv_vidc_init_module_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_rotation) for drv_vidc_set_rotation
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_init_get_scld_filter_h) for drv_param_init_get_scld_filter_h
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_init_get_scld_filter_v) for drv_param_init_get_scld_filter_v
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef0) for drv_vidc_set_scld_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef1) for drv_vidc_set_scld_hcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef0) for drv_vidc_set_scld_vcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef1) for drv_vidc_set_scld_vcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_p2r_hinitr) for drv_vidc_set_p2r_hinitr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_p2r_hinitb) for drv_vidc_set_p2r_hinitb
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_param_init.o(i.drv_param_p2r_filter_init) for drv_param_p2r_filter_init
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_p2r_hcoef0) for drv_vidc_set_p2r_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_mirror) for drv_vidc_set_mirror
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pu_ctrl) for drv_vidc_set_pu_ctrl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter) for drv_dsc_dec_convert_pps_rc_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_write_cmd_entry) refers to hal_internal_vsync.o(i.hal_internal_vsync_register_write_cmd_entry) for hal_internal_vsync_register_write_cmd_entry
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header) for drv_rxbr_set_ack_pkt_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) for hal_internal_vsync_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef0) for drv_vidc_set_scld_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef1) for drv_vidc_set_scld_hcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef0) for drv_vidc_set_scld_vcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef1) for drv_vidc_set_scld_vcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to drv_param_init.o(i.drv_param_init_set_scld_filter) for drv_param_init_set_scld_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) for hal_internal_vsync_set_sync_line
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg) for drv_rxbr_hline_rcv0_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_dcs_direct_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode) for hal_internal_vsync_set_dcs_direct_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) refers to drv_rxbr.o(i.drv_rxbr_set_cmd_filter) for drv_rxbr_set_cmd_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) for drv_dsi_rx_calc_ipi_tx_delay
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg) for drv_dsi_rx_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format) refers to drv_vidc.o(i.drv_vidc_update_src_format) for drv_vidc_update_src_format
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format) refers to drv_vidc.o(i.drv_vidc_set_pentile_swap) for drv_vidc_set_pentile_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dflti.o(.text) for __aeabi_i2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dmul.o(.text) for __aeabi_dmul
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to ddiv.o(.text) for __aeabi_ddiv
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to dflti.o(.text) for __aeabi_i2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to dmul.o(.text) for __aeabi_dmul
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to ddiv.o(.text) for __aeabi_ddiv
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) for hal_dsi_rx_ctrl_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk) for hal_intl_svs_update_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_src) for drv_crgu_set_rxbr_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_div) for drv_crgu_set_rxbr_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_dsco_src) for drv_crgu_set_dsco_src
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_dsco_src_div) for drv_crgu_set_dsco_src_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_dsc_core_div) for drv_crgu_set_dsc_core_div
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_te_waveform) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_te_waveform) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_dsi_rx.o(i.drv_dsi_rx_power_up) for drv_dsi_rx_power_up
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) for hal_internal_vsync_toggle_input_frame_rate
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) for hal_internal_sync_input_resolution_change
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution_ex) refers to hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) for hal_internal_sync_input_resolution_change_ex
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution_ex) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fscalb.o(.text) for __ARM_scalbnf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fflti.o(.text) for __aeabi_i2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to ffixi.o(.text) for __aeabi_f2iz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk) for drv_dsi_tx_set_video_chunk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing) for drv_dsi_tx_set_video_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to drv_phy_common.o(i.drv_phy_get_rate_para) for drv_phy_get_rate_para
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to ffixui.o(.text) for __aeabi_f2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) refers to hal_dsi_tx_ctrl.o(.conststring) for .conststring
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) for hal_lcdc_config_upscaler
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to drv_lcdc.o(i.drv_lcdc_config_src_parameter) for drv_lcdc_config_src_parameter
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic) refers to hal_internal_vsync.o(i.hal_internal_vsync_update_lcdc_addr) for hal_internal_vsync_update_lcdc_addr
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode_rcv_te) refers to hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) for hal_internal_sync_cmd_mode_rcv_te
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_param_init.o(i.drv_param_init_set_ccm) for drv_param_init_set_ccm
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.constdata) for .constdata
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) for hal_lcdc_config_upscaler
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) for hal_lcdc_config_remains
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_mode_init) for hal_dsi_tx_ctrl_draw_mode_init
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) for hal_dsi_tx_ctrl_set_rect_pixel_data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) for hal_lcdc_config_upscaler
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) for hal_lcdc_config_remains
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_mode_init) for hal_dsi_tx_ctrl_draw_mode_init
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_ulps_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) for drv_dsi_tx_phy_ulps_enter
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_ulps_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) for drv_dsi_tx_phy_ulps_exit
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) for hal_dsi_tx_ctrl_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_tx) for hal_internal_vsync_init_tx
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate) for hal_dsi_tx_config_params_for_lane_rate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate) for hal_dsi_tx_count_lane_rate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) for hal_dsi_tx_init_phy_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) for drv_dsi_tx_phy_test_setup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) for hal_lcdc_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) for hal_lcdc_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) for hal_dsi_tx_init_dpi_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) for hal_dsi_tx_init_data_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) for hal_dsi_tx_init_remains
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt) for hal_dsi_tx_init_interrupt
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready) for drv_dsi_tx_phy_status_ready
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload) for drv_dsi_tx_command_get_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) refers to drv_param_init.o(i.drv_param_init_set_ccm) for drv_param_init_set_ccm
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_pq_filter) refers to drv_lcdc.o(i.drv_lcdc_config_scale_up_coef) for drv_lcdc_config_scale_up_coef
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_pq_filter) refers to drv_param_init.o(i.drv_param_init_set_sclu_filter) for drv_param_init_set_sclu_filter
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness) refers to drv_lcdc.o(i.drv_lcdc_config_endianness) for drv_lcdc_config_endianness
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_lp_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd) for drv_dsi_tx_video_mode_set_lp_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb) for drv_lcdc_config_overwrite_rgb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp) refers to drv_lcdc.o(i.drv_lcdc_config_partial_display_enable) for drv_lcdc_config_partial_display_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area) refers to drv_lcdc.o(i.drv_lcdc_config_partial_display_area) for drv_lcdc_config_partial_display_area
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to dflti.o(.text) for __aeabi_i2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to dmul.o(.text) for __aeabi_dmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to ddiv.o(.text) for __aeabi_ddiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to dfixi.o(.text) for __aeabi_d2iz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_vpg) for drv_dsi_tx_set_vpg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker) for hal_dsi_tx_ctrl_draw_flicker
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard) for hal_dsi_tx_ctrl_draw_chessboard
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_enable_shadow_reg) for drv_lcdc_enable_shadow_reg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_check_video_auto_sync) for hal_internal_check_video_auto_sync
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_start) for drv_lcdc_start
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_set_video_hw_mode) for drv_lcdc_set_video_hw_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size) for drv_dsi_tx_edpi_cmd_size
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) for hal_dsi_tx_init_video_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode) for drv_dsi_tx_dpi_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity) for drv_dsi_tx_dpi_polarity
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time) for drv_dsi_tx_dpi_lpcmd_time
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_int) for drv_dsi_tx_config_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode) for drv_dsi_tx_phy_lane_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg) for drv_dsi_tx_phy_time_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_response_mode) for drv_dsi_tx_response_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div) for drv_dsi_tx_set_time_out_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg) for drv_dsi_tx_timeout_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp) for drv_dsi_tx_phy_clock_lane_auto_lp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg) for drv_dsi_tx_video_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack) for drv_dsi_tx_set_bta_ack
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd) for drv_dsi_tx_video_mode_set_lp_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_disable_hact_cmd) for drv_dsi_tx_video_mode_disable_hact_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks) for hal_dsi_tx_calc_video_chunks
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_header) for drv_dsi_tx_command_header
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) refers to drv_param_init.o(i.drv_param_init_get_ccm) for drv_param_init_get_ccm
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) refers to drv_lcdc.o(i.drv_lcdc_config_ccm) for drv_lcdc_config_ccm
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to hal_internal_vsync.o(i.hal_internal_check_video_auto_sync) for hal_internal_check_video_auto_sync
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_disp_mode) for drv_lcdc_config_disp_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_edpi_mode) for drv_lcdc_config_edpi_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_endianness) for drv_lcdc_config_endianness
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_thresh) for drv_lcdc_config_thresh
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_dpi_polarity) for drv_lcdc_config_dpi_polarity
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) refers to drv_lcdc.o(i.drv_lcdc_config_src_parameter) for drv_lcdc_config_src_parameter
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area) for hal_dsi_tx_ctrl_set_partial_disp_area
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp) for hal_dsi_tx_ctrl_set_partial_disp
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_lcdc.o(i.drv_lcdc_config_scale_up_step) for drv_lcdc_config_scale_up_step
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_param_init.o(i.drv_param_init_get_sclu_filter) for drv_param_init_get_sclu_filter
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_lcdc.o(i.drv_lcdc_config_scale_up_coef) for drv_lcdc_config_scale_up_coef
    hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler) for hal_lcdc_config_upscaler
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm) for hal_lcdc_config_ccm
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile) for hal_lcdc_config_rgb_to_pentile
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to drv_lcdc.o(i.drv_lcdc_config_bypass) for drv_lcdc_config_bypass
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains) for hal_lcdc_config_remains
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) for hal_lcdc_init_interrupt
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to drv_lcdc.o(i.drv_lcdc_set_prefetch) for drv_lcdc_set_prefetch
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dpi_pre_div) for drv_crgu_set_dpi_pre_div
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dpi_pre_src) for drv_crgu_set_dpi_pre_src
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dpi_mux_src) for drv_crgu_set_dpi_mux_src
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_lcdc.o(i.drv_lcdc_config_dpi_timing) for drv_lcdc_config_dpi_timing
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to hal_internal_vsync.o(i.hal_internal_check_video_auto_sync) for hal_internal_check_video_auto_sync
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to hal_internal_soft_sync.o(i.hal_intl_svs_init_tx) for hal_intl_svs_init_tx
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to cfrcmple.o(.text) for __aeabi_cfrcmple
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ffixi.o(.text) for __aeabi_f2iz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_lcdc_div) for drv_crgu_set_lcdc_div
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_lcdc_src) for drv_crgu_set_lcdc_src
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) for hal_tx_frame_rate_adjust
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to drv_lcdc.o(i.drv_lcdc_ctrl_flow) for drv_lcdc_ctrl_flow
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt) refers to drv_lcdc.o(i.drv_lcdc_config_int) for drv_lcdc_config_int
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to cfcmple.o(.text) for __aeabi_cfcmple
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_gpio.o(i.hal_gpio_ctrl_eint) refers to drv_gpio.o(i.drv_gpio_set_int) for drv_gpio_set_int
    hal_gpio.o(i.hal_gpio_ctrl_eint) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_get_input_data) refers to drv_gpio.o(i.drv_gpio_get_input_data) for drv_gpio_get_input_data
    hal_gpio.o(i.hal_gpio_get_int_type) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to drv_gpio.o(i.drv_gpio_get_pull_state) for drv_gpio_get_pull_state
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_eint) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group) for drv_sys_cfg_sel_gpio_group
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig) for drv_sys_cfg_sel_int_trig
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_init_eint) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_input) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_input) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_input) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_init_output) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_reg_eint_cb) refers to drv_gpio.o(i.drv_gpio_register_callback) for drv_gpio_register_callback
    hal_gpio.o(i.hal_gpio_reg_eint_cb) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_gpio.o(i.drv_gpio_register_ap_reset_callback) for drv_gpio_register_ap_reset_callback
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) for drv_sys_cfg_sel_ap_rst_trig
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to drv_gpio.o(i.drv_gpio_set_driving_strength) for drv_gpio_set_driving_strength
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode3) for drv_gpio_set_mode3
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode2) for drv_gpio_set_mode2
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode1) for drv_gpio_set_mode1
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode0) for drv_gpio_set_mode0
    hal_gpio.o(i.hal_gpio_set_mode) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_output_data) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to drv_gpio.o(i.drv_gpio_set_pull_state) for drv_gpio_set_pull_state
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to drv_gpio.o(i.drv_gpio_set_schmitt_trigger) for drv_gpio_set_schmitt_trigger
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to drv_gpio.o(i.drv_gpio_set_slew_rate) for drv_gpio_set_slew_rate
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to hal_gpio.o(.constdata) for .constdata
    hal_i2c_master.o(i.hal_i2c_m_deinit) refers to drv_i2c_master.o(i.drv_i2c_m_deinit) for drv_i2c_m_deinit
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_master.o(i.drv_i2c_master_init) for drv_i2c_master_init
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_master.o(i.drv_i2c1_set_callback) for drv_i2c1_set_callback
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_master.o(i.drv_i2c_m_enable_intr) for drv_i2c_m_enable_intr
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_dma.o(i.drv_i2c_dma_init) for drv_i2c_dma_init
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_dma.o(i.drv_i2c_enable_rx_dma) for drv_i2c_enable_rx_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to drv_i2c_dma.o(i.drv_i2c_enable_tx_dma) for drv_i2c_enable_tx_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_init) refers to hal_i2c_master.o(i.hal_i2c_master_irq_callback) for hal_i2c_master_irq_callback
    hal_i2c_master.o(i.hal_i2c_m_dma_read) refers to drv_i2c_dma.o(i.drv_i2c_master_read_dma) for drv_i2c_master_read_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_read) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_master.o(i.hal_i2c_m_dma_write) refers to drv_i2c_dma.o(i.drv_i2c_master_write_dma) for drv_i2c_master_write_dma
    hal_i2c_master.o(i.hal_i2c_m_dma_write) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_master.o(i.hal_i2c_m_set_high_impedance) refers to drv_i2c_master.o(i.drv_i2c_m_enable) for drv_i2c_m_enable
    hal_i2c_master.o(i.hal_i2c_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_master.o(i.hal_i2c_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_i2c_master.o(i.hal_i2c_m_transfer_complate) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_master.o(i.hal_i2c_master_irq_callback) refers to drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit) for drv_i2c_m_clear_it_pending_bit
    hal_i2c_master.o(i.hal_i2c_master_irq_callback) refers to hal_i2c_master.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to drv_i2c_slave.o(i.drv_i2c_s_set_intr) for drv_i2c_s_set_intr
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to drv_i2c_slave.o(i.drv_i2c_s_enable) for drv_i2c_s_enable
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_deinit) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to drv_i2c_dma.o(i.drv_i2c_slave_write_dma) for drv_i2c_slave_write_dma
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_dma_write) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_get_tx_byte_num) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c_slave_init) for drv_i2c_slave_init
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_master.o(i.drv_i2c1_set_callback) for drv_i2c1_set_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c_s_config_intr) for drv_i2c_s_config_intr
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c_s_set_intr) for drv_i2c_s_set_intr
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_dma.o(i.drv_i2c_dma_init) for drv_i2c_dma_init
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) for drv_i2c_set_dma_irq_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_dma.o(i.drv_i2c_enable_tx_dma) for drv_i2c_enable_tx_dma
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to drv_i2c_slave.o(i.drv_i2c0_set_callback) for drv_i2c0_set_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) for hal_i2c_slave_irq_callback
    hal_i2c_slave.o(i.hal_i2c_s_init) refers to hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback) for hal_i2c_s_dma_user_callback
    hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_complate) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_complate_clear) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_data) refers to drv_i2c_slave.o(i.drv_i2c_s_read_data) for drv_i2c_s_read_data
    hal_i2c_slave.o(i.hal_i2c_s_read_data) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_read_data) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_rxfifo_notempty) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    hal_i2c_slave.o(i.hal_i2c_s_rxfifo_notempty) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_rxfifo_notempty) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_sel) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_set_dma_tx_cycle) refers to drv_dma.o(i.drv_dma_enable_cycle) for drv_dma_enable_cycle
    hal_i2c_slave.o(i.hal_i2c_s_set_dma_tx_cycle) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_set_dma_tx_cycle) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to drv_i2c_slave.o(i.drv_i2c_s_enable) for drv_i2c_s_enable
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_s_set_transfer) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_write_complate) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_write_data) refers to drv_i2c_slave.o(i.drv_i2c_s_write_data) for drv_i2c_s_write_data
    hal_i2c_slave.o(i.hal_i2c_s_write_data) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_s_write_data) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit) for drv_i2c_s_clear_it_pending_bit
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to drv_i2c_slave.o(i.drv_i2c_s_write_data) for drv_i2c_s_write_data
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2c_slave_irq_callback) refers to hal_i2c_slave.o(.constdata) for .constdata
    hal_spi_master.o(i.hal_spi_m_callback) refers to drv_spi_dma.o(i.drv_spi_abort_dma) for drv_spi_abort_dma
    hal_spi_master.o(i.hal_spi_m_callback) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_clear_rxfifo) refers to drv_spi_master.o(i.drv_spi_m_read_data) for drv_spi_m_read_data
    hal_spi_master.o(i.hal_spi_m_deinit) refers to drv_spi_master.o(i.drv_spi_m_deinit) for drv_spi_m_deinit
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to hal_spi_master.o(i.hal_spi_m_gpio_init) for hal_spi_m_gpio_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_master.o(i.drv_spi_master_init) for drv_spi_master_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_dma_init) for drv_spi_dma_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_dma_ch6_init) for drv_spi_dma_ch6_init
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) for drv_spi_set_dma_irq_callback
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) for drv_spi_set_dma_ch6_irq_callback
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req) for drv_sys_cfg_set_dma_rx_req
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_master.o(i.drv_spi_m_enable_rx_dma) for drv_spi_m_enable_rx_dma
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    hal_spi_master.o(i.hal_spi_m_dma_init) refers to hal_spi_master.o(i.hal_spi_m_callback) for hal_spi_m_callback
    hal_spi_master.o(i.hal_spi_m_dma_read) refers to drv_spi_dma.o(i.drv_spim_dma_read) for drv_spim_dma_read
    hal_spi_master.o(i.hal_spi_m_dma_read) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_dma_write) refers to drv_spi_dma.o(i.drv_spim_dma_write) for drv_spim_dma_write
    hal_spi_master.o(i.hal_spi_m_dma_write) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_get_transfer_complate) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spi_m_gpio_init) refers to drv_spi_master.o(i.drv_spi_m_gpio_init) for drv_spi_m_gpio_init
    hal_spi_master.o(i.hal_spi_m_read_rxfifo) refers to drv_spi_master.o(i.drv_spi_m_read_data) for drv_spi_m_read_data
    hal_spi_master.o(i.hal_spi_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_spi_master.o(i.hal_spi_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    hal_spi_master.o(i.hal_spi_m_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_system.o(i.hal_system_deep_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode) for drv_pwr_enter_deep_sleep_mode
    hal_system.o(i.hal_system_disable_systick) refers to drv_common.o(i.drv_common_disable_systick) for drv_common_disable_systick
    hal_system.o(i.hal_system_enable_systick) refers to drv_common.o(i.drv_common_enable_systick) for drv_common_enable_systick
    hal_system.o(i.hal_system_get_tick) refers to drv_common.o(i.drv_common_get_tick) for drv_common_get_tick
    hal_system.o(i.hal_system_idle_mode) refers to drv_common.o(i.drv_common_idle_mode) for drv_common_idle_mode
    hal_system.o(i.hal_system_init) refers to drv_pwr.o(i.drv_pwr_set_system_clk_src) for drv_pwr_set_system_clk_src
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_set_ahb_src) for drv_crgu_set_ahb_src
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_set_ahb_pre_div) for drv_crgu_set_ahb_pre_div
    hal_system.o(i.hal_system_init) refers to irq_redirect .o(i.handle_init) for handle_init
    hal_system.o(i.hal_system_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int) for drv_sys_cfg_clear_all_int
    hal_system.o(i.hal_system_init) refers to drv_common.o(i.drv_common_system_init) for drv_common_system_init
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    hal_system.o(i.hal_system_init) refers to drv_pwr.o(i.drv_pwr_set_pvd_mode) for drv_pwr_set_pvd_mode
    hal_system.o(i.hal_system_init) refers to drv_common.o(.data) for g_system_clock
    hal_system.o(i.hal_system_init_console) refers to hal_uart.o(i.hal_uart_init) for hal_uart_init
    hal_system.o(i.hal_system_register_systick_cb) refers to drv_common.o(i.drv_common_systick_register_cb) for drv_common_systick_register_cb
    hal_system.o(i.hal_system_set_phy_calibration) refers to drv_phy_common.o(i.drv_phy_enable_calibration) for drv_phy_enable_calibration
    hal_system.o(i.hal_system_set_pvd) refers to drv_pwr.o(i.drv_pwr_set_pvd_mode) for drv_pwr_set_pvd_mode
    hal_system.o(i.hal_system_set_vcc) refers to drv_pwr.o(i.drv_pwr_set_cp_mode) for drv_pwr_set_cp_mode
    hal_system.o(i.hal_system_share_flash_mode) refers to drv_fls.o(i.drv_fls_gpio_connect) for drv_fls_gpio_connect
    hal_system.o(i.hal_system_share_flash_mode) refers to drv_fls.o(i.drv_fls_gpio_disconnect) for drv_fls_gpio_disconnect
    hal_system.o(i.hal_system_sleep_mode) refers to drv_crgu.o(i.drv_crgu_config_clocks) for drv_crgu_config_clocks
    tau_delay.o(i.delayMs) refers to tau_delay.o(i.delayUs) for delayUs
    tau_log.o(i.LOG_printf) refers to printfa.o(i.__0vsprintf) for vsprintf
    tau_log.o(i.LOG_printf) refers to printfa.o(i.__0printf) for __2printf
    tau_log.o(i.LOG_printf) refers to tau_log.o(.bss) for .bss
    tau_log.o(i.fgetc) refers to hal_uart.o(i.hal_uart_receive_blocking) for hal_uart_receive_blocking
    tau_log.o(i.fputc) refers to hal_uart.o(i.hal_uart_transmit_blocking) for hal_uart_transmit_blocking
    hal_uart.o(i.hal_uart_deinit) refers to drv_dma.o(i.drv_dma_deinit) for drv_dma_deinit
    hal_uart.o(i.hal_uart_deinit) refers to drv_uart.o(i.UART_Deinit) for UART_Deinit
    hal_uart.o(i.hal_uart_dmacallback) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_uart.o(i.hal_uart_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_uart.o(i.hal_uart_init) refers to drv_uart.o(i.UART_init) for UART_init
    hal_uart.o(i.hal_uart_init) refers to drv_common.o(.data) for g_system_clock
    hal_uart.o(i.hal_uart_init) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_receive_blocking) refers to drv_uart.o(i.UART_ReadBlocking) for UART_ReadBlocking
    hal_uart.o(i.hal_uart_receive_dma) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    hal_uart.o(i.hal_uart_receive_dma) refers to drv_uart_dma.o(i.UART_TransferCreateHandleDMA) for UART_TransferCreateHandleDMA
    hal_uart.o(i.hal_uart_receive_dma) refers to drv_uart_dma.o(i.UART_TransferReceiveDMA) for UART_TransferReceiveDMA
    hal_uart.o(i.hal_uart_receive_dma) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_receive_dma) refers to hal_uart.o(i.hal_uart_dmacallback) for hal_uart_dmacallback
    hal_uart.o(i.hal_uart_transmit_blocking) refers to drv_uart.o(i.UART_WriteBlocking) for UART_WriteBlocking
    hal_uart.o(i.hal_uart_transmit_dma) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    hal_uart.o(i.hal_uart_transmit_dma) refers to drv_uart_dma.o(i.UART_TransferCreateHandleDMA) for UART_TransferCreateHandleDMA
    hal_uart.o(i.hal_uart_transmit_dma) refers to drv_uart_dma.o(i.UART_TransferSendDMA) for UART_TransferSendDMA
    hal_uart.o(i.hal_uart_transmit_dma) refers to hal_uart.o(.bss) for .bss
    hal_uart.o(i.hal_uart_transmit_dma) refers to hal_uart.o(i.hal_uart_dmacallback) for hal_uart_dmacallback
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_param_init.o(i.drv_param_init_get_ccm) for drv_param_init_get_ccm
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_lcdc.o(i.drv_lcdc_config_ccm) for drv_lcdc_config_ccm
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to ddiv.o(.text) for __aeabi_ddiv
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to sqrt.o(i.sqrt) for sqrt
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to dmul.o(.text) for __aeabi_dmul
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to cdcmple.o(.text) for __aeabi_cdcmple
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.calc_framebuffer_setting) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to hal_internal_vsync.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_get_pkt_buf_error_status) for drv_rxbr_get_pkt_buf_error_status
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.dcs_sw_filter) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.dcs_sw_filter) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_check_video_auto_sync) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tear_mode) for hal_internal_vsync_get_tear_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_mode) for drv_memc_set_ltpo_mode
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_double_buffer) for drv_memc_set_double_buffer
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_active_height) for drv_memc_set_active_height
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_set_inten) for drv_memc_set_inten
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_internal_vsync.o(i.hal_internal_init_memc) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_rx_dcs_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) for dcs_packet_get_fifo_header
    hal_internal_vsync.o(i.hal_internal_rx_dcs_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) for dcs_packet_free_fifo_header
    hal_internal_vsync.o(i.hal_internal_rx_dcs_polling) refers to hal_internal_vsync.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_vsync.o(i.hal_internal_rx_dcs_polling) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_bta_status) for drv_dsi_rx_get_bta_status
    hal_internal_vsync.o(i.hal_internal_rx_dcs_polling) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.hal_internal_rx_dcs_polling) refers to hal_internal_vsync.o(i.drv_rxbr_get_status1) for drv_rxbr_get_status1
    hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) refers to drv_lcdc.o(i.drv_lcdc_start) for drv_lcdc_start
    hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) for hal_dsi_rx_ctrl_gen_a_tear_signal
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_delay.o(i.delayUs) for delayUs
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.hal_internal_init_memc) for hal_internal_init_memc
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to drv_lcdc.o(i.drv_lcdc_enable_shadow_reg) for drv_lcdc_enable_shadow_reg
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to tau_delay.o(i.delayMs) for delayMs
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal) for hal_dsi_rx_ctrl_gen_a_tear_signal
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to tau_delay.o(i.delayUs) for delayUs
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) for hal_vsync_reset_lcdc_scaler
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_internal_vsync.o(i.vsync_set_te_mode) for vsync_set_te_mode
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_tear_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_chip_info.o(i.drv_chip_rx_info_check) for drv_chip_rx_info_check
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_soft_sync.o(i.hal_intl_svs_init_rx) for hal_intl_svs_init_rx
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_rxbr.o(i.drv_rxbr_register_irq0_callback) for drv_rxbr_register_irq0_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_rxbr.o(i.drv_rxbr_register_irq1_callback) for drv_rxbr_register_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_vidc.o(i.drv_vidc_register_callback) for drv_vidc_register_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_init) for dcs_packet_fifo_init
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_gen_te) for soft_gen_te
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_gen_te_double_buffer) for soft_gen_te_double_buffer
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.rxbr_irq0_callback) for rxbr_irq0_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.rxbr_irq1_callback) for rxbr_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.vidc_callback) for vidc_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(i.calc_framebuffer_setting) for calc_framebuffer_setting
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_register_write_cmd_entry) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) refers to memseta.o(.text) for __aeabi_memset
    hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) refers to drv_rxbr.o(i.drv_rxbr_set_filter_regs) for drv_rxbr_set_filter_regs
    hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter) for hal_internal_vsync_set_auto_hw_filter
    hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_soft_sync.o(i.hal_intl_svs_deinit_tx) for hal_intl_svs_deinit_tx
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_soft_sync.o(i.hal_intl_svs_set_sync_coef) for hal_intl_svs_set_sync_coef
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(i.vsync_set_te_mode) for vsync_set_te_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_soft_sync.o(i.hal_intl_svs_deinit_tx) for hal_intl_svs_deinit_tx
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.vsync_set_te_mode) for vsync_set_te_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_soft_sync.o(i.hal_intl_svs_set_input_frate) for hal_intl_svs_set_input_frate
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg) for drv_rxbr_hline_rcv0_cfg
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_update_lcdc_addr) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dadd.o(.text) for __aeabi_dadd
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area) for hal_dsi_tx_ctrl_set_partial_disp_area
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp) for hal_dsi_tx_ctrl_set_partial_disp
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to drv_param_init.o(i.drv_param_init_get_sclu_filter) for drv_param_init_get_sclu_filter
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to drv_lcdc.o(i.drv_lcdc_config_scale_up_coef) for drv_lcdc_config_scale_up_coef
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_internal_vsync.o(i.hal_internal_init_memc) for hal_internal_init_memc
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(i.dcs_sw_filter) for dcs_sw_filter
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) for dcs_packet_fifo_alloc
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(i.hal_internal_rx_dcs_async_handler) for hal_internal_rx_dcs_async_handler
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_internal_vsync.o(i.rx_get_dcs_packet_data) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_rxbr.o(i.drv_rxbr_get_col_addr) for drv_rxbr_get_col_addr
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_rxbr.o(i.drv_rxbr_get_page_addr) for drv_rxbr_get_page_addr
    hal_internal_vsync.o(i.rx_partial_update) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_dsc_dec.o(i.drv_dsc_dec_get_nslc) for drv_dsc_dec_get_nslc
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_crgu.o(i.drv_crgu_set_dsco_src) for drv_crgu_set_dsco_src
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_crgu.o(i.drv_crgu_set_dsco_src_div) for drv_crgu_set_dsco_src_div
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_crgu.o(i.drv_crgu_set_dsc_core_div) for drv_crgu_set_dsc_core_div
    hal_internal_vsync.o(i.rx_partial_update) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rx_partial_update) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(i.rx_get_dcs_packet_data) for rx_get_dcs_packet_data
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(i.rx_receive_pps) for rx_receive_pps
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(i.drv_rxbr_get_status1) for drv_rxbr_get_status1
    hal_internal_vsync.o(i.rx_receive_packet) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_bta_status) for drv_dsi_rx_get_bta_status
    hal_internal_vsync.o(i.rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_get_pkt_buf_error_status) for drv_rxbr_get_pkt_buf_error_status
    hal_internal_vsync.o(i.rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rx_receive_packet) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rx_receive_pps) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.rx_receive_pps) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rx_receive_pps) refers to hal_internal_vsync.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter) for drv_dsc_dec_convert_pps_rc_parameter
    hal_internal_vsync.o(i.rx_receive_pps) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_internal_vsync.o(i.rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps) for drv_dsc_dec_set_u8_pps
    hal_internal_vsync.o(i.rx_receive_pps) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.rx_receive_pps) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_int_source) for drv_rxbr_get_int_source
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.rx_receive_packet) for rx_receive_packet
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.vpre_err_reset) for vpre_err_reset
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(i.rx_partial_update) for rx_partial_update
    hal_internal_vsync.o(i.rxbr_irq0_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_int_source) for drv_rxbr_get_int_source
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_soft_sync.o(i.hal_intl_svs_handle) for hal_intl_svs_handle
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.vpre_err_reset) for vpre_err_reset
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_lcdc.o(i.drv_lcdc_start) for drv_lcdc_start
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_memc.o(i.drv_memc_set_double_buffer_reverse) for drv_memc_set_double_buffer_reverse
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.soft_gen_te_double_buffer) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_gen_te_double_buffer) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_get_irq_status) for drv_vidc_get_irq_status
    hal_internal_vsync.o(i.vidc_callback) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite) for drv_lcdc_config_overwrite
    hal_internal_vsync.o(i.vidc_callback) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_clear_irq) for drv_vidc_clear_irq
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_internal_vsync.o(i.vidc_callback) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_crgu.o(i.drv_crgu_config_reset_modules) for drv_crgu_config_reset_modules
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps) for drv_dsc_dec_set_u8_pps
    hal_internal_vsync.o(i.vpre_err_reset) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to drv_lcdc.o(i.drv_lcdc_ctrl_flow) for drv_lcdc_ctrl_flow
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vsync_set_te_mode) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(.data) refers to hal_internal_vsync.o(.bss) for sg_te_info
    drv_common.o(i.app_HardFault_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_common.o(i.app_SysTick_Handler) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_enable_systick) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_common.o(i.drv_common_enable_systick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_get_tick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_system_init) refers to drv_chip_info.o(i.drv_chip_info_init) for drv_chip_info_init
    drv_common.o(i.drv_common_systick_register_cb) refers to drv_common.o(.data) for .data
    drv_dma.o(i.app_dma_irq_handler) refers to drv_dma.o(i.drv_dma_irq_handler) for drv_dma_irq_handler
    drv_dma.o(i.drv_dma_abort_transfer) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_abort_transfer) refers to drv_dma.o(i.drv_dma_disenable_channel_interrupts) for drv_dma_disenable_channel_interrupts
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_disenable_channel_interrupts) for drv_dma_disenable_channel_interrupts
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_clear_flag) for drv_dma_clear_flag
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_set_ccr) for drv_dma_set_ccr
    drv_dma.o(i.drv_dma_ahb_init) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_dma.o(i.drv_dma_clear_flag) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.drv_dma_create_handle) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dma.o(i.drv_dma_disenable_channel_interrupts) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.drv_dma_enable_channel_interrupts) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dma.o(i.drv_dma_enable_cycle) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_get_remaining_bytes) refers to drv_dma.o(i.drv_dma_channel_is_active) for drv_dma_channel_is_active
    drv_dma.o(i.drv_dma_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dma.o(i.drv_dma_init) refers to drv_dma.o(i.drv_dma_ahb_init) for drv_dma_ahb_init
    drv_dma.o(i.drv_dma_irq_handler) refers to drv_dma.o(i.drv_dma_get_channel_flag) for drv_dma_get_channel_flag
    drv_dma.o(i.drv_dma_irq_handler) refers to drv_dma.o(i.drv_dma_clear_flag) for drv_dma_clear_flag
    drv_dma.o(i.drv_dma_irq_handler) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_m2m_init) refers to memseta.o(.text) for __aeabi_memclr4
    drv_dma.o(i.drv_dma_m2m_init) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    drv_dma.o(i.drv_dma_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_dma.o(i.drv_dma_set_burst) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_dma.o(i.drv_dma_set_transfer) refers to drv_dma.o(i.drv_dma_set_burst) for drv_dma_set_burst
    drv_dma.o(i.drv_dma_start_transfer) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    drv_dma.o(i.drv_dma_start_transfer) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_fls.o(i.drv_fls_gpio_connect) refers to drv_fls.o(i.drv_fls_gpio_disconnect) for drv_fls_gpio_disconnect
    drv_fls.o(i.drv_fls_gpio_disconnect) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_EnableClk) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_busy_pending) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    drv_fls.o(i.fls_de_init) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    drv_fls.o(i.fls_de_init) refers to drv_dma.o(i.drv_dma_clear_flag) for drv_dma_clear_flag
    drv_fls.o(i.fls_de_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_disable_it) refers to drv_fls.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_fls.o(i.fls_disable_it) refers to drv_fls.o(i.fls_set_mc_irq_mask) for fls_set_mc_irq_mask
    drv_fls.o(i.fls_enable_it) refers to drv_fls.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_fls.o(i.fls_enable_it) refers to drv_fls.o(i.fls_set_mc_irq_mask) for fls_set_mc_irq_mask
    drv_fls.o(i.fls_init) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_fls.o(i.fls_init) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_spi_init) for fls_spi_init
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_ctrl_cfg_init) for fls_ctrl_cfg_init
    drv_fls.o(i.fls_init) refers to drv_fls.o(i.fls_set_tuning) for fls_set_tuning
    drv_fls.o(i.fls_init) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls.o(i.fls_read_byte_data) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls.o(i.fls_read_cmd) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_enable_it) for fls_enable_it
    drv_fls.o(i.fls_read_cmd_it) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_set_mc_irq_mask) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_fls.o(i.fls_set_mc_irq_mask) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_set_write) for fls_set_write
    drv_fls.o(i.fls_write_byte_data) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_set_write) for fls_set_write
    drv_fls.o(i.fls_write_cmd) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect) for drv_ap_rst_trig_edge_detect
    drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_get_pull_state) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_register_ap_reset_callback) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.drv_gpio_register_callback) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_set_driving_strength) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.drv_gpio_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_gpio.o(i.drv_gpio_set_pull_state) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_set_schmitt_trigger) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_gpio.o(i.drv_gpio_set_slew_rate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_i2c_dma.o(i.drv_i2c_dma_callback) refers to drv_i2c_dma.o(.data) for .data
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_i2c_master.o(i.drv_i2c_m_enable) for drv_i2c_m_enable
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req) for drv_sys_cfg_set_dma_rx_req
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_dma.o(i.drv_dma_set_transfer) for drv_dma_set_transfer
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_i2c_dma.o(i.drv_i2c_master_read_dma) refers to drv_i2c_dma.o(i.drv_i2c_master_write_read_cmd) for drv_i2c_master_write_read_cmd
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_dma.o(i.drv_dma_set_transfer) for drv_dma_set_transfer
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_i2c_dma.o(i.drv_i2c_master_write_dma) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_i2c_dma.o(.data) for .data
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_i2c_dma.o(.bss) for .bss
    drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback) refers to drv_i2c_dma.o(i.drv_i2c_dma_callback) for drv_i2c_dma_callback
    drv_i2c_dma.o(i.drv_i2c_slave_write_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_i2c_master.o(i.app_I2C1_IRQn_Handler) refers to drv_i2c_master.o(.data) for .data
    drv_i2c_master.o(i.drv_i2c1_set_callback) refers to drv_i2c_master.o(.data) for .data
    drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_deinit) refers to drv_i2c_master.o(i.drv_i2c_m_disable_intr) for drv_i2c_m_disable_intr
    drv_i2c_master.o(i.drv_i2c_m_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_i2c_master.o(i.drv_i2c_m_deinit) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_i2c_master.o(i.drv_i2c_m_deinit) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_enable_intr) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_read_data) refers to drv_i2c_master.o(i.drv_i2c_m_get_fifo_status) for drv_i2c_m_get_fifo_status
    drv_i2c_master.o(i.drv_i2c_m_set_sys_mask) refers to drv_i2c_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_i2c_master.o(i.drv_i2c_m_write_data) refers to drv_i2c_master.o(i.drv_i2c_m_get_fifo_status) for drv_i2c_m_get_fifo_status
    drv_i2c_master.o(i.drv_i2c_master_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_i2c_master.o(i.drv_i2c_master_init) refers to drv_common.o(.data) for g_system_clock
    drv_i2c_slave.o(i.app_I2C0_IRQn_Handler) refers to drv_i2c_slave.o(.data) for .data
    drv_i2c_slave.o(i.drv_i2c0_set_callback) refers to drv_i2c_slave.o(.data) for .data
    drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_i2c_slave.o(i.drv_i2c_s_read_data) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    drv_i2c_slave.o(i.drv_i2c_s_set_intr) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_i2c_slave.o(i.drv_i2c_s_set_intr) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_i2c_slave.o(i.drv_i2c_s_write_data) refers to drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status) for drv_i2c_s_get_fifo_status
    drv_i2c_slave.o(i.drv_i2c_slave_init) refers to drv_i2c_slave.o(i.drv_i2c_s_enable) for drv_i2c_s_enable
    drv_param_init.o(i.drv_param_init_get_ccm) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_get_scld_filter_h) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_get_scld_filter_v) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_get_sclu_filter) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_set_ccm) refers to memcpya.o(.text) for __aeabi_memcpy4
    drv_param_init.o(i.drv_param_init_set_ccm) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_set_scld_filter) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_init_set_sclu_filter) refers to drv_param_init.o(.data) for .data
    drv_param_init.o(i.drv_param_p2r_filter_init) refers to drv_param_init.o(.constdata) for .constdata
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_dma.o(i.drv_dma_disenable_channel) for drv_dma_disenable_channel
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_dma.o(i.drv_dma_disenable_channel_interrupts) for drv_dma_disenable_channel_interrupts
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_master.o(i.drv_spi_m_enable_rx_dma) for drv_spi_m_enable_rx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_slave.o(i.drv_spi_s_enable_tx_dma) for drv_spi_s_enable_tx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_slave.o(i.drv_spi_s_enable_rx_dma) for drv_spi_s_enable_rx_dma
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_abort_dma) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_dma.o(i.drv_spi_dma_callback) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_dma_ch6_init) refers to drv_spi_dma.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_dma.o(i.drv_spi_dma_ch6_init) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_dma_init) refers to drv_spi_dma.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_dma.o(i.drv_spi_dma_init) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback) refers to drv_spi_dma.o(i.drv_spi_dma_callback) for drv_spi_dma_callback
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) refers to drv_spi_dma.o(i.drv_spi_dma_callback) for drv_spi_dma_callback
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_spi_master.o(i.drv_spi_m_enable_rx_dma) for drv_spi_m_enable_rx_dma
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_spi_dma.o(i.drv_spim_dma_read) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_spi_master.o(i.drv_spi_m_enable_tx_dma) for drv_spi_m_enable_tx_dma
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_dma.o(i.drv_dma_enable_channel_interrupts) for drv_dma_enable_channel_interrupts
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_spi_dma.o(i.drv_spim_dma_write) refers to drv_spi_dma.o(.data) for .data
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_spi_slave.o(i.drv_spi_s_enable_tx_dma) for drv_spi_s_enable_tx_dma
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_dma.o(i.drv_dma_enable_channel) for drv_dma_enable_channel
    drv_spi_dma.o(i.drv_spis_dma_write) refers to drv_spi_dma.o(.bss) for .bss
    drv_spi_master.o(i.app_SPIM_IRQn_Handler) refers to drv_spi_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_master.o(i.app_SPIM_IRQn_Handler) refers to drv_spi_master.o(.data) for .data
    drv_spi_master.o(i.drv_spi_m_deinit) refers to drv_spi_master.o(i.drv_spi_m_switch_sclk) for drv_spi_m_switch_sclk
    drv_spi_master.o(i.drv_spi_m_disable_int) refers to drv_spi_master.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    drv_spi_master.o(i.drv_spi_m_set_intr_callback) refers to drv_spi_master.o(.data) for .data
    drv_spi_master.o(i.drv_spi_master_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_spi_master.o(i.drv_spi_master_init) refers to drv_common.o(.data) for g_system_clock
    drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig) for drv_sys_cfg_sel_ap_rst_lvl_trig
    drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect) refers to drv_sys_cfg.o(.data) for .data
    drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig) for drv_sys_cfg_sel_ap_rst_lvl_trig
    drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) refers to drv_sys_cfg.o(.data) for .data
    hal_internal_soft_sync.o(i.hal_intl_svs_deinit_rx) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_soft_sync.o(i.hal_intl_svs_deinit_rx) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.hal_intl_svs_deinit_rx) refers to hal_internal_soft_sync.o(i.svs_wait_start) for svs_wait_start
    hal_internal_soft_sync.o(i.hal_intl_svs_deinit_tx) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.hal_intl_svs_handle) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.hal_intl_svs_init_rx) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_soft_sync.o(i.hal_intl_svs_init_rx) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_soft_sync.o(i.hal_intl_svs_init_rx) refers to hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk) for hal_intl_svs_update_rxbr_clk
    hal_internal_soft_sync.o(i.hal_intl_svs_init_rx) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.hal_intl_svs_init_rx) refers to hal_internal_soft_sync.o(i.svs_wait_start) for svs_wait_start
    hal_internal_soft_sync.o(i.hal_intl_svs_init_tx) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.hal_intl_svs_set_input_frate) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_soft_sync.o(i.hal_intl_svs_set_input_frate) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_soft_sync.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_soft_sync.o(i.svs_wait_start) for svs_wait_start
    hal_internal_soft_sync.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_soft_sync.o(i.svs_waite_fr_stab) for svs_waite_fr_stab
    hal_internal_soft_sync.o(i.hal_intl_svs_set_sync_coef) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk) refers to dmul.o(.text) for __aeabi_dmul
    hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.svs_direct_mode_setting) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_soft_sync.o(i.svs_direct_mode_setting) refers to hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting) for hal_internal_sync_get_fb_setting
    hal_internal_soft_sync.o(i.svs_direct_mode_setting) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_soft_sync.o(i.svs_direct_mode_setting) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg) for drv_rxbr_hline_rcv1_cfg
    hal_internal_soft_sync.o(i.svs_direct_mode_setting) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.svs_get_rel_intv) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_soft_sync.o(i.svs_get_rel_intv) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to hal_internal_soft_sync.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to f2d.o(.text) for __aeabi_f2d
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to dadd.o(.text) for __aeabi_dadd
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_soft_sync.o(i.svs_sync_handle) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.svs_wait_start) refers to hal_internal_soft_sync.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_soft_sync.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_get_clk) for drv_rxbr_get_clk
    hal_internal_soft_sync.o(i.svs_wait_start) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_soft_sync.o(i.svs_wait_start) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_soft_sync.o(i.svs_wait_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_internal_soft_sync.o(i.svs_wait_start) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_soft_sync.o(i.svs_wait_start) refers to f2d.o(.text) for __aeabi_f2d
    hal_internal_soft_sync.o(i.svs_wait_start) refers to ceil.o(i.ceil) for ceil
    hal_internal_soft_sync.o(i.svs_wait_start) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_soft_sync.o(i.svs_wait_start) refers to hal_internal_soft_sync.o(i.svs_direct_mode_setting) for svs_direct_mode_setting
    hal_internal_soft_sync.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg) for drv_rxbr_hline_rcv1_cfg
    hal_internal_soft_sync.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_soft_sync.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_soft_sync.o(i.svs_wait_start) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_soft_sync.o(i.svs_wait_start) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.svs_wait_start) refers to hal_internal_soft_sync.o(i.svs_waite_fr_stab) for svs_waite_fr_stab
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to hal_internal_soft_sync.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to ffixui.o(.text) for __aeabi_f2uiz
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to hal_internal_soft_sync.o(.bss) for .bss
    hal_internal_soft_sync.o(i.svs_waite_fr_stab) refers to hal_internal_soft_sync.o(i.svs_sync_handle) for svs_sync_handle
    drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to ffltui.o(.text) for __aeabi_ui2f
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fdiv.o(.text) for __aeabi_fdiv
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fmul.o(.text) for __aeabi_fmul
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) for drv_dsi_rx_get_color_bpp
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc) for drv_dsi_rx_get_color_pcc
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fadd.o(.text) for __aeabi_fadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to cfrcmple.o(.text) for __aeabi_cfrcmple
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to f2d.o(.text) for __aeabi_f2d
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dadd.o(.text) for __aeabi_dadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dfixui.o(.text) for __aeabi_d2uiz
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte) for drv_rx_phy_test_write_1_byte
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to drv_dsi_rx.o(i.drv_rx_phy_test_read) for drv_rx_phy_test_read
    drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap) refers to drv_chip_info.o(i.drv_chip_info_get_info) for drv_chip_info_get_info
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_get_rate_para) for drv_phy_get_rate_para
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_get_calibration) for drv_phy_get_calibration
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_clear) for drv_rx_phy_test_clear
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte) for drv_rx_phy_test_write_1_byte
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte) for drv_rx_phy_test_write_2_byte
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_chip_info.o(i.drv_chip_info_get_info) for drv_chip_info_get_info
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_dsi_rx.o(i.drv_rx_phy_test_lock) for drv_rx_phy_test_lock
    drv_dsi_rx.o(i.drv_rx_phy_test_clear) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_rx.o(i.drv_rx_phy_test_lock) refers to drv_phy_common.o(i.drv_phy_test_lock) for drv_phy_test_lock
    drv_dsi_rx.o(i.drv_rx_phy_test_read) refers to drv_phy_common.o(i.drv_phy_test_read) for drv_phy_test_read
    drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_1_byte) for drv_phy_test_write_1_byte
    drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_2_byte) for drv_phy_test_write_2_byte
    drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) for drv_tx_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to drv_dsi_tx.o(i.drv_tx_phy_test_read) for drv_tx_phy_test_read
    drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_get_rate_para) for drv_phy_get_rate_para
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_get_pll_para) for drv_phy_get_pll_para
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_get_calibration) for drv_phy_get_calibration
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_enter) for drv_tx_phy_test_enter
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_crgu.o(i.drv_crgu_set_mipi_ref_src) for drv_crgu_set_mipi_ref_src
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_crgu.o(i.drv_crgu_set_mipi_cfg_src) for drv_crgu_set_mipi_cfg_src
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_clear) for drv_tx_phy_test_clear
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) for drv_tx_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte) for drv_tx_phy_test_write_2_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_code) for drv_tx_phy_test_write_code
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_exit) for drv_tx_phy_test_exit
    drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) for drv_tx_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_version) for drv_dsi_tx_version
    drv_dsi_tx.o(i.drv_dsi_tx_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_tx.o(i.drv_dsi_tx_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dsi_tx.o(i.drv_tx_phy_test_clear) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_tx.o(i.drv_tx_phy_test_read) refers to drv_phy_common.o(i.drv_phy_test_read) for drv_phy_test_read
    drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_1_byte) for drv_phy_test_write_1_byte
    drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_2_byte) for drv_phy_test_write_2_byte
    drv_dsi_tx.o(i.drv_tx_phy_test_write_code) refers to drv_phy_common.o(i.drv_phy_test_write_code) for drv_phy_test_write_code
    drv_lcdc.o(i.drv_lcdc_config_src_parameter) refers to drv_lcdc.o(i.drv_lcdc_config_input_size) for drv_lcdc_config_input_size
    drv_lcdc.o(i.drv_lcdc_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_lcdc.o(i.drv_lcdc_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_memc.o(i.app_MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_get_status) for drv_memc_get_status
    drv_memc.o(i.app_MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_clear_status) for drv_memc_clear_status
    drv_memc.o(i.app_MEMC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_rxbr.o(i.app_ADC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.app_ADC_IRQn_Handler) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.app_VPRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.app_VPRE_IRQn_Handler) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_EnableIRQ) for __NVIC_EnableIRQ
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_rxbr.o(i.drv_rxbr_register_irq0_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_register_irq1_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_set_cmd_filter) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_rxbr.o(i.drv_rxbr_soft_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_vidc.o(i.app_VIDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.app_VIDC_IRQn_Handler) refers to drv_vidc.o(.data) for .data
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_vidc.o(i.drv_vidc_register_callback) refers to drv_vidc.o(.data) for .data
    irq_redirect .o(i.ADC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.AP_NRESET_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.DMA_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT0_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT1_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT2_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT3_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT4_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT5_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT6_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.EXTI_INT7_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.FLSCTRL_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.HardFault_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.I2C0_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.I2C1_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.LCDC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.MEMC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.MIPI_RX_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.MIPI_TX_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.PWMDET_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SPIM_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SPIS_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SWIRE_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.SysTick_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER0_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER1_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER2_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.TIMER3_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.UART_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.VIDC_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.VPRE_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.WDG_IRQn_Handler) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.handle_init) refers to irq_redirect .o(.ARM.__AT_0x00070100) for .ARM.__AT_0x00070100
    irq_redirect .o(i.handle_init) refers to drv_common.o(i.app_SysTick_Handler) for app_SysTick_Handler
    irq_redirect .o(i.handle_init) refers to hal_internal_vsync.o(i.app_LCDC_IRQn_Handler) for app_LCDC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler) for app_MIPI_RX_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler) for app_MIPI_TX_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_dma.o(i.app_dma_irq_handler) for app_dma_irq_handler
    irq_redirect .o(i.handle_init) refers to norflash.o(i.app_fls_ctrl_Handler) for app_fls_ctrl_Handler
    irq_redirect .o(i.handle_init) refers to drv_i2c_slave.o(i.app_I2C0_IRQn_Handler) for app_I2C0_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_i2c_master.o(i.app_I2C1_IRQn_Handler) for app_I2C1_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to hal_spi_slave.o(i.app_SPIS_IRQn_Handler) for app_SPIS_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_spi_master.o(i.app_SPIM_IRQn_Handler) for app_SPIM_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_rxbr.o(i.app_VPRE_IRQn_Handler) for app_VPRE_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_rxbr.o(i.app_ADC_IRQn_Handler) for app_ADC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_vidc.o(i.app_VIDC_IRQn_Handler) for app_VIDC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_memc.o(i.app_MEMC_IRQn_Handler) for app_MEMC_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER0_IRQn_Handler) for app_TIMER0_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER1_IRQn_Handler) for app_TIMER1_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER2_IRQn_Handler) for app_TIMER2_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_timer.o(i.app_TIMER3_IRQn_Handler) for app_TIMER3_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_wdg.o(i.app_WDG_IRQn_Handler) for app_WDG_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_uart.o(i.app_UART_IRQn_Handler) for app_UART_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_pwm.o(i.app_PWMDET_IRQn_Handler) for app_PWMDET_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_swire.o(i.app_SWIRE_IRQn_Handler) for app_SWIRE_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_AP_NRESET_IRQn_Handler) for app_AP_NRESET_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler) for app_EXTI_INT0_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler) for app_EXTI_INT1_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler) for app_EXTI_INT2_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler) for app_EXTI_INT3_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler) for app_EXTI_INT4_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler) for app_EXTI_INT5_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler) for app_EXTI_INT6_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler) for app_EXTI_INT7_IRQn_Handler
    irq_redirect .o(i.handle_init) refers to drv_common.o(i.app_HardFault_Handler) for app_HardFault_Handler
    drv_efuse.o(i.drv_efuse_enter_inactive) refers to drv_efuse.o(i.drv_efuse_int_enable) for drv_efuse_int_enable
    drv_efuse.o(i.drv_efuse_read) refers to drv_efuse.o(i.drv_efuse_read_req) for drv_efuse_read_req
    drv_efuse.o(i.drv_efuse_write) refers to drv_efuse.o(i.drv_efuse_write_req) for drv_efuse_write_req
    drv_phy_common.o(i.drv_phy_enable_calibration) refers to drv_phy_common.o(.data) for .data
    drv_phy_common.o(i.drv_phy_get_calibration) refers to drv_chip_info.o(i.drv_chip_info_get_info) for drv_chip_info_get_info
    drv_phy_common.o(i.drv_phy_get_calibration) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_phy_common.o(i.drv_phy_get_calibration) refers to drv_phy_common.o(.data) for .data
    drv_phy_common.o(i.drv_phy_get_pll_para) refers to drv_phy_common.o(.constdata) for .constdata
    drv_phy_common.o(i.drv_phy_get_rate_para) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_phy_common.o(i.drv_phy_get_rate_para) refers to drv_phy_common.o(.constdata) for .constdata
    drv_phy_common.o(i.drv_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_code) for drv_phy_test_write_code
    drv_phy_common.o(i.drv_phy_test_write_1_byte) refers to drv_phy_common.o(i.drv_phy_test_write_data) for drv_phy_test_write_data
    drv_phy_common.o(i.drv_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_code) for drv_phy_test_write_code
    drv_phy_common.o(i.drv_phy_test_write_2_byte) refers to drv_phy_common.o(i.drv_phy_test_write_data) for drv_phy_test_write_data
    drv_chip_info.o(i.drv_chip_info_get_info) refers to drv_chip_info.o(.data) for .data
    drv_chip_info.o(i.drv_chip_info_init) refers to drv_efuse.o(i.drv_efuse_enter_inactive) for drv_efuse_enter_inactive
    drv_chip_info.o(i.drv_chip_info_init) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_chip_info.o(i.drv_chip_info_init) refers to drv_chip_info.o(.data) for .data
    drv_chip_info.o(i.drv_chip_rx_info_check) refers to printfa.o(i.__0printf) for __2printf
    drv_chip_info.o(i.drv_chip_rx_info_check) refers to tau_log.o(i.LOG_printf) for LOG_printf
    drv_chip_info.o(i.drv_chip_rx_info_check) refers to drv_chip_info.o(.data) for .data
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to drv_efuse.o(i.drv_efuse_enter_inactive) for drv_efuse_enter_inactive
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to printfa.o(i.__0printf) for __2printf
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to hal_spi_slave.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_spi_slave.o(i.app_SPIS_IRQn_Handler) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_spi_slave.o(i.hal_spi_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    hal_spi_slave.o(i.hal_spi_s_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_abort) refers to drv_spi_dma.o(i.drv_spi_abort_dma) for drv_spi_abort_dma
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start) refers to drv_dma.o(i.drv_dma_enable_cycle) for drv_dma_enable_cycle
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start) refers to drv_spi_dma.o(i.drv_spis_dma_write) for drv_spis_dma_write
    hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_deinit) refers to drv_spi_slave.o(i.drv_spi_s_deinit) for drv_spi_s_deinit
    hal_spi_slave.o(i.hal_spi_slave_enable) refers to drv_spi_slave.o(i.drv_spi_s_enable_int) for drv_spi_s_enable_int
    hal_spi_slave.o(i.hal_spi_slave_enable) refers to tau_log.o(i.LOG_printf) for LOG_printf
    hal_spi_slave.o(i.hal_spi_slave_enable) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_gpio_init) refers to drv_spi_slave.o(i.drv_spi_s_gpio_init) for drv_spi_s_gpio_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to hal_spi_slave.o(i.hal_spi_slave_gpio_init) for hal_spi_slave_gpio_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_slave.o(i.drv_spi_slave_init) for drv_spi_slave_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_dma.o(i.drv_spi_dma_init) for drv_spi_dma_init
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_dma.o(i.drv_spi_set_dma_irq_callback) for drv_spi_set_dma_irq_callback
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_spi_slave.o(i.drv_spi_s_enable_tx_dma) for drv_spi_s_enable_tx_dma
    hal_spi_slave.o(i.hal_spi_slave_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    hal_spi_slave.o(i.hal_spi_slave_init) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_read_data) refers to drv_spi_slave.o(i.drv_spi_s_read_data) for drv_spi_s_read_data
    hal_spi_slave.o(i.hal_spi_slave_register_callback) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_reset_tx) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_set_auto_rx_buffer) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_set_auto_tx_buffer) refers to hal_spi_slave.o(.bss) for .bss
    hal_spi_slave.o(i.hal_spi_slave_write_data) refers to drv_spi_slave.o(i.drv_spi_s_write_data) for drv_spi_s_write_data
    norflash.o(i.app_fls_ctrl_Handler) refers to drv_fls.o(i.fls_clr_interrupt_flag) for fls_clr_interrupt_flag
    norflash.o(i.app_fls_ctrl_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    norflash.o(i.app_fls_ctrl_Handler) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_best_cfg_init) refers to drv_fls.o(i.fls_spi_init) for fls_spi_init
    norflash.o(i.norflash_best_cfg_init) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_check_id) refers to norflash.o(i.norflash_read_id) for norflash_read_id
    norflash.o(i.norflash_check_id) refers to tau_delay.o(i.delayUs) for delayUs
    norflash.o(i.norflash_check_id) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dma_callback) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dma_read) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_transfer_create_handle_dma) for fls_transfer_create_handle_dma
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_dma_read_prepare) for fls_dma_read_prepare
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_transfer_dma) for fls_transfer_dma
    norflash.o(i.norflash_dma_read) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    norflash.o(i.norflash_dma_read) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dma_read) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_dma_read) refers to norflash.o(i.norflash_dma_callback) for norflash_dma_callback
    norflash.o(i.norflash_dma_write) refers to drv_dma.o(i.drv_dma_create_handle) for drv_dma_create_handle
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_transfer_create_handle_dma) for fls_transfer_create_handle_dma
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_switch_fls_spi) for norflash_switch_fls_spi
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_dma_write_prepare) for fls_dma_write_prepare
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_transfer_dma) for fls_transfer_dma
    norflash.o(i.norflash_dma_write) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    norflash.o(i.norflash_dma_write) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_dma_write) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_dma_write) refers to norflash.o(i.norflash_dma_callback) for norflash_dma_callback
    norflash.o(i.norflash_dma_write) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_dual_read) refers to drv_fls.o(i.fls_ddat_enable) for fls_ddat_enable
    norflash.o(i.norflash_dual_read) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_dual_read) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_switch_fls_spi) for norflash_switch_fls_spi
    norflash.o(i.norflash_dual_write) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_dual_write) refers to drv_fls.o(i.fls_ddat_enable) for fls_ddat_enable
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_dual_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_en4b) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_read_config_reg) for norflash_read_config_reg
    norflash.o(i.norflash_en4b) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_en_quad) refers to norflash.o(i.norflash_en_quad_check) for norflash_en_quad_check
    norflash.o(i.norflash_en_quad) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_en_quad) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_en_quad) refers to drv_fls.o(i.fls_busy_pending) for fls_busy_pending
    norflash.o(i.norflash_en_quad) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(i.norflash_get_dual_hstatus) for norflash_get_dual_hstatus
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(i.norflash_get_hstatus) for norflash_get_hstatus
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_en_quad_check) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_erase_block) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_erase_block) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_erase_block) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_erase_block) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_erase_chip) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_erase_chip) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_erase_chip) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_erase_sector) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_erase_sector) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_erase_sector) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_erase_sector) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_ex4b) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_read_config_reg) for norflash_read_config_reg
    norflash.o(i.norflash_ex4b) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_exit_quad) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_exit_quad) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_exit_quad) refers to norflash.o(i.norflash_en_quad_check) for norflash_en_quad_check
    norflash.o(i.norflash_exit_quad) refers to drv_fls.o(i.fls_busy_pending) for fls_busy_pending
    norflash.o(i.norflash_exit_quad) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_get_dual_hstatus) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_get_dual_hstatus) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_get_dual_hstatus) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_get_hstatus) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_get_hstatus) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_get_hstatus) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_get_status) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_get_status) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_get_status) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_get_default_spi_config) for fls_get_default_spi_config
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_get_default_fls_config) for fls_get_default_fls_config
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_get_default_tuning) for fls_get_default_tuning
    norflash.o(i.norflash_init) refers to drv_fls.o(i.fls_init) for fls_init
    norflash.o(i.norflash_init) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_init) refers to drv_fls.o(.data) for g_fls_tuning
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_qdat_enable) for fls_qdat_enable
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_qadr_enable) for fls_qadr_enable
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_qcmd_enable) for fls_qcmd_enable
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_quad_read) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_switch_fls_spi) for norflash_switch_fls_spi
    norflash.o(i.norflash_quad_write) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_quad_write) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_quad_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_read) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_read_config_reg) refers to drv_fls.o(i.fls_read_byte_data) for fls_read_byte_data
    norflash.o(i.norflash_read_id) refers to drv_fls.o(i.fls_read_cmd) for fls_read_cmd
    norflash.o(i.norflash_read_uid) refers to memseta.o(.text) for __aeabi_memclr4
    norflash.o(i.norflash_read_uid) refers to drv_fls.o(i.fls_read_cmd) for fls_read_cmd
    norflash.o(i.norflash_read_uid) refers to memcpya.o(.text) for __aeabi_memcpy
    norflash.o(i.norflash_set_best_cfg) refers to memseta.o(.text) for __aeabi_memclr4
    norflash.o(i.norflash_set_best_read_cfg) refers to norflash.o(i.norflash_en_quad) for norflash_en_quad
    norflash.o(i.norflash_set_best_read_cfg) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_set_best_read_cfg) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_set_best_write_cfg) refers to norflash.o(i.norflash_en_quad) for norflash_en_quad
    norflash.o(i.norflash_set_best_write_cfg) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_set_best_write_cfg) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_single_mode) for fls_single_mode
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_set_addr_dummy) for fls_set_addr_dummy
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_ddat_enable) for fls_ddat_enable
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_qdat_enable) for fls_qdat_enable
    norflash.o(i.norflash_switch_fls_spi) refers to drv_fls.o(i.fls_qadr_enable) for fls_qadr_enable
    norflash.o(i.norflash_write) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_write) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_write) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    norflash.o(i.norflash_write_disable) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_write_disable) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write_disable) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_write_disable) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_write_enable) refers to drv_fls.o(i.fls_write_cmd) for fls_write_cmd
    norflash.o(i.norflash_write_enable) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write_enable) refers to norflash.o(.bss) for .bss
    norflash.o(i.norflash_write_enable) refers to norflash.o(.data) for .data
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_write_enable) for norflash_write_enable
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_big_end_enable) for norflash_big_end_enable
    norflash.o(i.norflash_write_endian_scr) refers to drv_fls.o(i.fls_en_scr) for fls_en_scr
    norflash.o(i.norflash_write_endian_scr) refers to drv_fls.o(i.fls_write_byte_data) for fls_write_byte_data
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_big_end_clear) for norflash_big_end_clear
    norflash.o(i.norflash_write_endian_scr) refers to drv_fls.o(i.fls_scr_clear) for fls_scr_clear
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_get_status) for norflash_get_status
    norflash.o(i.norflash_write_endian_scr) refers to norflash.o(i.norflash_write_disable) for norflash_write_disable
    drv_fls_dma.o(i.fls_abort_dma) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_fls_dma.o(i.fls_abort_dma) refers to drv_fls_dma.o(i.fls_dma_disable) for fls_dma_disable
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_set_read) for fls_set_read
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls_dma.o(i.fls_dma_enable) for fls_dma_enable
    drv_fls_dma.o(i.fls_dma_read_prepare) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_clear_irq_status) for fls_clear_irq_status
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_swrst) for fls_swrst
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_set_write) for fls_set_write
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls_dma.o(i.fls_dma_enable) for fls_dma_enable
    drv_fls_dma.o(i.fls_dma_write_prepare) refers to drv_fls.o(i.fls_spi_start) for fls_spi_start
    drv_fls_dma.o(i.fls_read_dmacallback) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to memseta.o(.text) for __aeabi_memclr4
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_fls_dma.o(.data) for .data
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_fls_dma.o(i.fls_read_dmacallback) for fls_read_dmacallback
    drv_fls_dma.o(i.fls_transfer_create_handle_dma) refers to drv_fls_dma.o(i.fls_write_dmacallback) for fls_write_dmacallback
    drv_fls_dma.o(i.fls_transfer_dma) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_fls_dma.o(i.fls_transfer_dma) refers to drv_dma.o(i.drv_dma_start_transfer) for drv_dma_start_transfer
    drv_fls_dma.o(i.fls_transfer_get_receive_count_dma) refers to drv_dma.o(i.drv_dma_get_remaining_bytes) for drv_dma_get_remaining_bytes
    drv_fls_dma.o(i.fls_write_dmacallback) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_pwm.o(i.app_PWMDET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_pwm.o(i.app_PWMDET_IRQn_Handler) refers to drv_pwm.o(.data) for .data
    drv_pwm.o(i.drv_pwm_in_register_callback) refers to drv_pwm.o(.data) for .data
    drv_pwm.o(i.drv_pwm_in_set_sys_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_pwm.o(i.drv_pwm_in_set_sys_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_spi_slave.o(i.drv_spi_s_deinit) refers to drv_spi_slave.o(i.drv_spi_s_switch_sclk) for drv_spi_s_switch_sclk
    drv_swire.o(i.app_SWIRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_swire.o(i.app_SWIRE_IRQn_Handler) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    drv_swire.o(i.app_SWIRE_IRQn_Handler) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_register_callback) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_swire.o(i.drv_swire_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_timer.o(i.app_TIMER0_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.app_TIMER1_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.app_TIMER2_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.app_TIMER3_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_timer.o(i.drv_timer_enable) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_get_instance) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_get_prescaler) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_get_status) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_clear_status_flags) for drv_timer_clear_status_flags
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_register_callback) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_compare_val) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_timer.o(i.drv_timer_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_repeat) refers to drv_timer.o(.data) for .data
    drv_uart.o(i.UART0_IRQ_Handle) refers to drv_uart.o(i.UART_TransferHandleIRQ) for UART_TransferHandleIRQ
    drv_uart.o(i.UART0_IRQ_Handle) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_uart.o(i.UART0_IRQ_Handle) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_AbortReceive) refers to drv_uart.o(i.UART_Disable_IT) for UART_Disable_IT
    drv_uart.o(i.UART_AbortReceive) refers to drv_uart.o(i.UART_ResetRxFIFO) for UART_ResetRxFIFO
    drv_uart.o(i.UART_AbortSend) refers to drv_uart.o(i.UART_Disable_IT) for UART_Disable_IT
    drv_uart.o(i.UART_AbortSend) refers to drv_uart.o(i.UART_ResetTxFIFO) for UART_ResetTxFIFO
    drv_uart.o(i.UART_Deinit) refers to drv_uart.o(i.UART_SwitchSCLK) for UART_SwitchSCLK
    drv_uart.o(i.UART_Disable_IT) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_Disable_IT) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.UART_Disable_IT) refers to drv_uart.o(.constdata) for .constdata
    drv_uart.o(i.UART_EnableDma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req) for drv_sys_cfg_set_dma_rx_req
    drv_uart.o(i.UART_EnableDma) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req) for drv_sys_cfg_set_dma_tx_req
    drv_uart.o(i.UART_Enable_IT) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_Enable_IT) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.UART_GetDefaultConfig) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.UART_GetDefaultConfig) refers to drv_common.o(.data) for g_system_clock
    drv_uart.o(i.UART_GetFIFO_Ctrl) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_GetFIFO_Ctrl) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_ResetRxFIFO) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_ResetRxFIFO) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_ResetTxFIFO) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_ResetTxFIFO) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_SetBaudRate) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_uart.o(i.UART_SwitchSCLK) refers to drv_crgu.o(i.drv_crgu_set_clock) for drv_crgu_set_clock
    drv_uart.o(i.UART_TransferCreateHandle) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_TransferCreateHandle) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.UART_TransferCreateHandle) refers to drv_uart.o(i.UART_Enable_IT) for UART_Enable_IT
    drv_uart.o(i.UART_TransferCreateHandle) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.UART_TransferHandleIRQ) refers to drv_uart.o(i.UART_ResetRxFIFO) for UART_ResetRxFIFO
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_DisableDma) for UART_DisableDma
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_SwitchSCLK) for UART_SwitchSCLK
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart.o(i.UART_init) refers to drv_uart.o(i.UART_SetBaudRate) for UART_SetBaudRate
    drv_uart.o(i.UART_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.UART_init) refers to drv_uart.o(.data) for .data
    drv_uart.o(i.app_UART_IRQn_Handler) refers to drv_uart.o(i.UART0_IRQ_Handle) for UART0_IRQ_Handle
    drv_uart_dma.o(i.UART_DMAInit) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart_dma.o(i.UART_DMAInit) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    drv_uart_dma.o(i.UART_TransferAbortReceiveDMA) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_uart_dma.o(i.UART_TransferAbortSendDMA) refers to drv_dma.o(i.drv_dma_abort_transfer) for drv_dma_abort_transfer
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart.o(i.UART_GetInstance) for UART_GetInstance
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart.o(i.UART_EnableDma) for UART_EnableDma
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(i.UART_DMAInit) for UART_DMAInit
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_dma.o(i.drv_dma_set_callback) for drv_dma_set_callback
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(.data) for .data
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(i.UART_TransferReceiveDMACallback) for UART_TransferReceiveDMACallback
    drv_uart_dma.o(i.UART_TransferCreateHandleDMA) refers to drv_uart_dma.o(i.UART_TransferSendDMACallback) for UART_TransferSendDMACallback
    drv_uart_dma.o(i.UART_TransferGetReceiveCountDMA) refers to drv_dma.o(i.drv_dma_get_remaining_bytes) for drv_dma_get_remaining_bytes
    drv_uart_dma.o(i.UART_TransferReceiveDMA) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_uart_dma.o(i.UART_TransferReceiveDMA) refers to drv_uart.o(i.UART_EnableDma) for UART_EnableDma
    drv_uart_dma.o(i.UART_TransferReceiveDMA) refers to drv_dma.o(i.drv_dma_start_transfer) for drv_dma_start_transfer
    drv_uart_dma.o(i.UART_TransferSendDMA) refers to drv_dma.o(i.drv_dma_prepar_transfer) for drv_dma_prepar_transfer
    drv_uart_dma.o(i.UART_TransferSendDMA) refers to drv_uart.o(i.UART_EnableDma) for UART_EnableDma
    drv_uart_dma.o(i.UART_TransferSendDMA) refers to drv_dma.o(i.drv_dma_start_transfer) for drv_dma_start_transfer
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_set_int) for drv_wdg_set_int
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_clear_counter) for drv_wdg_clear_counter
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_read_edge_flag) for drv_wdg_read_edge_flag
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_clear_edge_flag) for drv_wdg_clear_edge_flag
    drv_wdg.o(i.app_WDG_IRQn_Handler) refers to drv_wdg.o(.data) for .data
    drv_wdg.o(i.drv_wdg_register_callback) refers to drv_wdg.o(.data) for .data
    drv_wdg.o(i.drv_wdg_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_wdg.o(i.drv_wdg_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_wdg.o(i.drv_wdg_set_repeat) refers to drv_wdg.o(.data) for .data
    dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_fifo_init) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_size) refers to dcs_packet_fifo.o(.bss) for .bss
    ceil.o(i.__softfp_ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.__softfp_ceil) refers to ceil.o(i.ceil) for ceil
    ceil.o(i.ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.ceil) refers to dadd.o(.text) for __aeabi_dadd
    ceil.o(i.ceil) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    sqrt.o(i.__softfp_sqrt) refers (Special) to iusefp.o(.text) for __I$use$fp
    sqrt.o(i.__softfp_sqrt) refers to dsqrt.o(.text) for _dsqrt
    sqrt.o(i.__softfp_sqrt) refers to errno.o(i.__set_errno) for __set_errno
    sqrt.o(i.sqrt) refers (Special) to iusefp.o(.text) for __I$use$fp
    sqrt.o(i.sqrt) refers to dsqrt.o(.text) for _dsqrt
    sqrt.o(i.sqrt) refers to errno.o(i.__set_errno) for __set_errno
    sqrt_x.o(i.____softfp_sqrt$lsc) refers (Special) to iusefp.o(.text) for __I$use$fp
    sqrt_x.o(i.____softfp_sqrt$lsc) refers to cdcmple.o(.text) for __aeabi_cdcmple
    sqrt_x.o(i.____softfp_sqrt$lsc) refers to errno.o(i.__set_errno) for __set_errno
    sqrt_x.o(i.____softfp_sqrt$lsc) refers to dsqrt.o(.text) for _dsqrt
    sqrt_x.o(i.__sqrt$lsc) refers (Special) to iusefp.o(.text) for __I$use$fp
    sqrt_x.o(i.__sqrt$lsc) refers to cdcmple.o(.text) for __aeabi_cdcmple
    sqrt_x.o(i.__sqrt$lsc) refers to errno.o(i.__set_errno) for __set_errno
    sqrt_x.o(i.__sqrt$lsc) refers to dsqrt.o(.text) for _dsqrt
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry10a.o(.ARM.Collect$$$$0000000D) for __rt_final_cpp
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry11a.o(.ARM.Collect$$$$0000000F) for __rt_final_exit
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry7b.o(.ARM.Collect$$$$00000008) for _main_clock
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry8b.o(.ARM.Collect$$$$0000000A) for _main_cpp_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry9a.o(.ARM.Collect$$$$0000000B) for _main_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry5.o(.ARM.Collect$$$$00000004) for _main_scatterload
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry2.o(.ARM.Collect$$$$00000001) for _main_stk
    idiv.o(.text) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfb.o(i.__0fprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0fprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0printf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printfb.o(i.__0vfprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vfprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printf0.o(i.__0fprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0fprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0printf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf0.o(i.__0vfprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vfprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf1.o(i.__0fprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0fprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0printf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i.__0vfprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vfprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf2.o(i.__0fprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0fprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0printf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf2.o(i.__0vfprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vfprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf3.o(i.__0fprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0fprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0printf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i.__0vfprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vfprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf4.o(i.__0fprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0fprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0printf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i.__0vfprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vfprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf5.o(i.__0fprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0fprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0printf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i.__0vfprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vfprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf6.o(i.__0fprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0fprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0printf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i.__0vfprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vfprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i._printf_core) refers to printf6.o(i._printf_pre_padding) for _printf_pre_padding
    printf6.o(i._printf_core) refers to printf6.o(i._printf_post_padding) for _printf_post_padding
    printf6.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf7.o(i.__0fprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0fprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0printf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i.__0vfprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vfprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i._printf_core) refers to printf7.o(i._printf_pre_padding) for _printf_pre_padding
    printf7.o(i._printf_core) refers to printf7.o(i._printf_post_padding) for _printf_post_padding
    printf7.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf8.o(i.__0fprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0fprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0printf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i.__0vfprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vfprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i._printf_core) refers to printf8.o(i._printf_pre_padding) for _printf_pre_padding
    printf8.o(i._printf_core) refers to printf8.o(i._printf_post_padding) for _printf_post_padding
    printf8.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i.__0fprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0fprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0fprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0printf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0printf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0snprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0snprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0snprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0sprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0sprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0sprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i.__0vfprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vfprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vfprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0vsnprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0vsprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i._fp_digits) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._fp_digits) refers to dmul.o(.text) for __aeabi_dmul
    printfa.o(i._fp_digits) refers to ddiv.o(.text) for __aeabi_ddiv
    printfa.o(i._fp_digits) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    printfa.o(i._fp_digits) refers to dadd.o(.text) for __aeabi_dadd
    printfa.o(i._fp_digits) refers to dfixul.o(.text) for __aeabi_d2ulz
    printfa.o(i._fp_digits) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_core) refers to printfa.o(i._printf_pre_padding) for _printf_pre_padding
    printfa.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers to printfa.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i._printf_core) refers to printfa.o(i._fp_digits) for _fp_digits
    printfa.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfa.o(i._printf_post_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_pre_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._snputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._sputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    fmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers to fepilogue.o(.text) for _float_round
    fscalb.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    dadd.o(.text) refers to llsshr.o(.text) for __aeabi_lasr
    dadd.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dmul.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ddiv.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ddiv.o(.text) refers to depilogue.o(.text) for _double_round
    fflti.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fflti.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    ffltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ffltui.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    dflti.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dflti.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dfltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfltui.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ffixi.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ffixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixi.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixi.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixui.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    f2d.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    cdcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    cfcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    cfrcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    entry2.o(.ARM.Collect$$$$00000001) refers to entry2.o(.ARM.Collect$$$$00002712) for __lit__00000000
    entry2.o(.ARM.Collect$$$$00002712) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    entry5.o(.ARM.Collect$$$$00000004) refers to init.o(.text) for __scatterload
    entry9a.o(.ARM.Collect$$$$0000000B) refers to main.o(i.main) for main
    entry9b.o(.ARM.Collect$$$$0000000C) refers to main.o(i.main) for main
    uldiv.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    uldiv.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    errno.o(i.__aeabi_errno_addr) refers to errno.o(.data) for .data
    errno.o(i.__read_errno) refers to errno.o(.data) for .data
    errno.o(i.__set_errno) refers to errno.o(.data) for .data
    depilogue.o(.text) refers to depilogue.o(i.__ARM_clz) for __ARM_clz
    depilogue.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dsqrt.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dsqrt.o(.text) refers to depilogue.o(.text) for _double_round
    dfixul.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixul.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    init.o(.text) refers to entry5.o(.ARM.Collect$$$$00000004) for __main_after_scatterload


==============================================================================

Removing Unused input sections from the image.

    Removing main.o(.rev16_text), (4 bytes).
    Removing main.o(.revsh_text), (4 bytes).
    Removing ap_demo.o(.rev16_text), (4 bytes).
    Removing ap_demo.o(.revsh_text), (4 bytes).
    Removing ap_demo.o(i.tp_heartbeat_exec), (104 bytes).
    Removing ap_demo.o(i.tp_power_up_restart), (36 bytes).
    Removing ap_demo.o(.data), (1 bytes).
    Removing ap_demo.o(.data), (2 bytes).
    Removing ap_demo.o(.data), (1 bytes).
    Removing ap_demo.o(.data), (256 bytes).
    Removing ap_demo.o(.data), (256 bytes).
    Removing ap_demo.o(.data), (2 bytes).
    Removing ap_demo.o(.data), (2 bytes).
    Removing ap_demo.o(.data), (2 bytes).
    Removing ap_demo.o(.data), (2 bytes).
    Removing app_tp_transfer.o(.rev16_text), (4 bytes).
    Removing app_tp_transfer.o(.revsh_text), (4 bytes).
    Removing app_tp_transfer.o(i.S20_Start_init), (356 bytes).
    Removing app_tp_transfer.o(i.app_tp_I2C_init), (36 bytes).
    Removing app_tp_transfer.o(i.app_tp_i2cs_callback), (64 bytes).
    Removing app_tp_transfer.o(i.app_tp_init), (64 bytes).
    Removing app_tp_transfer.o(i.app_tp_m_read), (32 bytes).
    Removing app_tp_transfer.o(i.app_tp_m_transfer_complate), (8 bytes).
    Removing app_tp_transfer.o(i.app_tp_m_write), (8 bytes).
    Removing app_tp_transfer.o(i.app_tp_phone_clear_reset_on), (12 bytes).
    Removing app_tp_transfer.o(i.app_tp_phone_reset_on), (12 bytes).
    Removing app_tp_transfer.o(i.app_tp_s_read), (8 bytes).
    Removing app_tp_transfer.o(i.app_tp_s_transfer_complate), (26 bytes).
    Removing app_tp_transfer.o(i.app_tp_s_write), (8 bytes).
    Removing app_tp_transfer.o(i.app_tp_screen_init), (48 bytes).
    Removing app_tp_transfer.o(i.app_tp_screen_int_callback), (12 bytes).
    Removing app_tp_transfer.o(i.app_tp_transfer_screen_const), (64 bytes).
    Removing app_tp_transfer.o(i.app_tp_transfer_screen_int), (276 bytes).
    Removing app_tp_transfer.o(i.app_tp_transfer_screen_start), (24 bytes).
    Removing app_tp_transfer.o(.bss), (400 bytes).
    Removing app_tp_transfer.o(.data), (23 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (5 bytes).
    Removing app_tp_transfer.o(.data), (6 bytes).
    Removing app_tp_transfer.o(.data), (2 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (4 bytes).
    Removing app_tp_transfer.o(.data), (4 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (3 bytes).
    Removing app_tp_transfer.o(.data), (1 bytes).
    Removing app_tp_transfer.o(.data), (2 bytes).
    Removing app_tp_transfer.o(.data), (2 bytes).
    Removing app_tp_st_touch.o(.rev16_text), (4 bytes).
    Removing app_tp_st_touch.o(.revsh_text), (4 bytes).
    Removing app_tp_st_touch.o(i.CRC16_2), (64 bytes).
    Removing app_tp_st_touch.o(i.ap_set_tp_calibration_04), (152 bytes).
    Removing app_tp_st_touch.o(i.ap_tp_st_touch_calibration), (176 bytes).
    Removing app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_F3), (26 bytes).
    Removing app_tp_st_touch.o(i.ap_tp_st_touch_error_handler_FF), (32 bytes).
    Removing app_tp_st_touch.o(i.ap_tp_st_touch_get_calibration_success_mark), (168 bytes).
    Removing app_tp_st_touch.o(i.ap_tp_st_touch_hardware_reset), (188 bytes).
    Removing app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_init), (28 bytes).
    Removing app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event), (148 bytes).
    Removing app_tp_st_touch.o(i.ap_tp_st_touch_scan_point_record_event_exec), (80 bytes).
    Removing app_tp_st_touch.o(i.ap_tp_st_touch_simulate_finger_release_event), (52 bytes).
    Removing app_tp_st_touch.o(i.ap_tp_st_touch_software_reset), (112 bytes).
    Removing app_tp_st_touch.o(i.app_tp_calibration_exec), (168 bytes).
    Removing app_tp_st_touch.o(i.app_tp_phone_analysis_data_for_wake_up), (64 bytes).
    Removing app_tp_st_touch.o(i.app_tp_screen_analysis_wake_up), (160 bytes).
    Removing app_tp_st_touch.o(i.app_tp_screen_analysis_wake_up_exec), (192 bytes).
    Removing app_tp_st_touch.o(.bss), (28 bytes).
    Removing app_tp_st_touch.o(.constdata), (32 bytes).
    Removing board.o(.rev16_text), (4 bytes).
    Removing board.o(.revsh_text), (4 bytes).
    Removing startup_armcm0.o(HEAP), (3072 bytes).
    Removing app_tp_for_custom_s8.o(.rev16_text), (4 bytes).
    Removing app_tp_for_custom_s8.o(.revsh_text), (4 bytes).
    Removing app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data), (852 bytes).
    Removing app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const), (56 bytes).
    Removing app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int), (684 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (5286 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (16 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (1120 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (1120 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (288 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (1 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (3 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (3 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (1 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (3 bytes).
    Removing app_tp_for_custom_s8.o(.data), (5 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (48 bytes).
    Removing app_tp_for_custom_s8.o(.data), (64 bytes).
    Removing app_tp_for_custom_s8.o(.data), (3 bytes).
    Removing app_tp_for_custom_s8.o(.data), (2 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing app_tp_for_custom_s8.o(.data), (32 bytes).
    Removing app_tp_for_custom_s8.o(.data), (1 bytes).
    Removing hal_dsi_rx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd), (88 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_short_cmd), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_crop_video), (228 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit), (176 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init), (48 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern), (216 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en), (16 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_hight_performan_mode), (100 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_write_cmd_entry), (10 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle), (40 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_dcs_direct_mode), (8 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter), (40 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_tear_mode), (52 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pentile_format), (56 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data), (148 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rect_pixel_data), (268 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk), (80 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_sw_tear_mode), (52 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_te_waveform), (52 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop), (60 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate), (10 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution_ex), (32 bytes).
    Removing hal_dsi_tx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_crop_pic), (148 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode_rcv_te), (10 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit), (132 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_chessboard), (280 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flicker), (172 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_mode_init), (30 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_ulps_mode), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_ulps_mode), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd), (140 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle), (28 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_pq_filter), (28 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_lp_cmd), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite), (16 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_rect_pixel_data), (272 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg), (80 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop), (68 bytes).
    Removing hal_dsi_tx_ctrl.o(.constdata), (36 bytes).
    Removing hal_gpio.o(.rev16_text), (4 bytes).
    Removing hal_gpio.o(.revsh_text), (4 bytes).
    Removing hal_gpio.o(i.hal_gpio_ctrl_eint), (24 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_int_type), (20 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_pull_state), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_init_eint), (64 bytes).
    Removing hal_gpio.o(i.hal_gpio_reg_eint_cb), (24 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_ap_reset_int), (80 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_driving_strength), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_output_data_ex), (36 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_schmitt_trigger), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_slew_rate), (32 bytes).
    Removing hal_i2c_master.o(.rev16_text), (4 bytes).
    Removing hal_i2c_master.o(.revsh_text), (4 bytes).
    Removing hal_i2c_master.o(i.hal_i2c_m_deinit), (8 bytes).
    Removing hal_i2c_master.o(i.hal_i2c_m_dma_init), (108 bytes).
    Removing hal_i2c_master.o(i.hal_i2c_m_dma_read), (32 bytes).
    Removing hal_i2c_master.o(i.hal_i2c_m_dma_write), (28 bytes).
    Removing hal_i2c_master.o(i.hal_i2c_m_set_high_impedance), (46 bytes).
    Removing hal_i2c_master.o(i.hal_i2c_m_transfer_complate), (12 bytes).
    Removing hal_i2c_master.o(i.hal_i2c_master_irq_callback), (32 bytes).
    Removing hal_i2c_master.o(.data), (1 bytes).
    Removing hal_i2c_slave.o(.rev16_text), (4 bytes).
    Removing hal_i2c_slave.o(.revsh_text), (4 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_deinit), (88 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_dma_user_callback), (16 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_dma_write), (76 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_get_tx_byte_num), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_init), (200 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_nonblocking_read), (20 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_read_complate), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_read_complate_clear), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_read_data), (32 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_rxfifo_notempty), (40 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_sel), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_set_dma_tx_cycle), (36 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_set_high_impedance), (88 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_set_transfer), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_write_complate), (12 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_s_write_data), (32 bytes).
    Removing hal_i2c_slave.o(i.hal_i2c_slave_irq_callback), (372 bytes).
    Removing hal_i2c_slave.o(.constdata), (32 bytes).
    Removing hal_i2c_slave.o(.data), (32 bytes).
    Removing hal_spi_master.o(.rev16_text), (4 bytes).
    Removing hal_spi_master.o(.revsh_text), (4 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_callback), (24 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_clear_rxfifo), (14 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_deinit), (10 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_dma_init), (104 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_dma_read), (36 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_dma_write), (40 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_get_transfer_complate), (36 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_gpio_init), (8 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_read_rxfifo), (28 bytes).
    Removing hal_spi_master.o(i.hal_spi_m_set_high_impedance), (100 bytes).
    Removing hal_spi_master.o(.data), (1 bytes).
    Removing hal_system.o(.rev16_text), (4 bytes).
    Removing hal_system.o(.revsh_text), (4 bytes).
    Removing hal_system.o(i.hal_system_clear_debug_state), (10 bytes).
    Removing hal_system.o(i.hal_system_deep_sleep_mode), (8 bytes).
    Removing hal_system.o(i.hal_system_disable_systick), (8 bytes).
    Removing hal_system.o(i.hal_system_get_debug_state), (8 bytes).
    Removing hal_system.o(i.hal_system_idle_mode), (8 bytes).
    Removing hal_system.o(i.hal_system_register_systick_cb), (8 bytes).
    Removing hal_system.o(i.hal_system_reset_chip), (32 bytes).
    Removing hal_system.o(i.hal_system_set_pvd), (8 bytes).
    Removing hal_system.o(i.hal_system_set_vcc), (8 bytes).
    Removing hal_system.o(i.hal_system_share_flash_mode), (20 bytes).
    Removing hal_system.o(i.hal_system_sleep_mode), (48 bytes).
    Removing tau_delay.o(.rev16_text), (4 bytes).
    Removing tau_delay.o(.revsh_text), (4 bytes).
    Removing tau_log.o(.rev16_text), (4 bytes).
    Removing tau_log.o(.revsh_text), (4 bytes).
    Removing tau_log.o(i.fgetc), (22 bytes).
    Removing hal_uart.o(.rev16_text), (4 bytes).
    Removing hal_uart.o(.revsh_text), (4 bytes).
    Removing hal_uart.o(i.hal_uart_deinit), (28 bytes).
    Removing hal_uart.o(i.hal_uart_dmacallback), (36 bytes).
    Removing hal_uart.o(i.hal_uart_receive_blocking), (16 bytes).
    Removing hal_uart.o(i.hal_uart_receive_dma), (76 bytes).
    Removing hal_uart.o(i.hal_uart_transmit_dma), (76 bytes).
    Removing hal_internal_vsync.o(.rev16_text), (4 bytes).
    Removing hal_internal_vsync.o(.revsh_text), (4 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te), (168 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change_ex), (468 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual), (512 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state), (12 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_register_write_cmd_entry), (12 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_set_dcs_direct_mode), (48 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate), (152 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_update_lcdc_addr), (48 bytes).
    Removing hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler), (476 bytes).
    Removing drv_common.o(.rev16_text), (4 bytes).
    Removing drv_common.o(.revsh_text), (4 bytes).
    Removing drv_common.o(i.drv_common_disable_systick), (20 bytes).
    Removing drv_common.o(i.drv_common_idle_mode), (40 bytes).
    Removing drv_common.o(i.drv_common_systick_register_cb), (12 bytes).
    Removing drv_crgu.o(.rev16_text), (4 bytes).
    Removing drv_crgu.o(.revsh_text), (4 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_all_reset_flags), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_reset_flag), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_config_clocks), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_config_clocks_div), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_config_clocks_src), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_ana_clk_status), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_clocks), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_fpga_id), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_mipi_ref_src), (16 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_reset_flag), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_system_clk), (28 bytes).
    Removing drv_crgu.o(i.drv_crgu_reset_chip), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_200m_scan_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_300m_scan_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_abp0_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_adc_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_adc_src), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_apb1_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_apb2_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_fls_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_fls_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_monitor_div), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_monitor_src), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_swire_div), (20 bytes).
    Removing drv_dma.o(.rev16_text), (4 bytes).
    Removing drv_dma.o(.revsh_text), (4 bytes).
    Removing drv_dma.o(i.drv_dma_abort_transfer), (32 bytes).
    Removing drv_dma.o(i.drv_dma_ahb_init), (74 bytes).
    Removing drv_dma.o(i.drv_dma_channel_is_active), (20 bytes).
    Removing drv_dma.o(i.drv_dma_create_handle), (28 bytes).
    Removing drv_dma.o(i.drv_dma_deinit), (32 bytes).
    Removing drv_dma.o(i.drv_dma_disenable_channel), (16 bytes).
    Removing drv_dma.o(i.drv_dma_disenable_channel_interrupts), (24 bytes).
    Removing drv_dma.o(i.drv_dma_enable_channel), (16 bytes).
    Removing drv_dma.o(i.drv_dma_enable_channel_interrupts), (36 bytes).
    Removing drv_dma.o(i.drv_dma_enable_cycle), (44 bytes).
    Removing drv_dma.o(i.drv_dma_get_remaining_bytes), (32 bytes).
    Removing drv_dma.o(i.drv_dma_init), (24 bytes).
    Removing drv_dma.o(i.drv_dma_m2m_init), (72 bytes).
    Removing drv_dma.o(i.drv_dma_prepar_transfer), (18 bytes).
    Removing drv_dma.o(i.drv_dma_reset), (10 bytes).
    Removing drv_dma.o(i.drv_dma_set_burst), (26 bytes).
    Removing drv_dma.o(i.drv_dma_set_callback), (6 bytes).
    Removing drv_dma.o(i.drv_dma_set_ccr), (114 bytes).
    Removing drv_dma.o(i.drv_dma_set_transfer), (68 bytes).
    Removing drv_dma.o(i.drv_dma_start_transfer), (32 bytes).
    Removing drv_fls.o(.rev16_text), (4 bytes).
    Removing drv_fls.o(.revsh_text), (4 bytes).
    Removing drv_fls.o(i.__NVIC_DisableIRQ), (32 bytes).
    Removing drv_fls.o(i.drv_fls_gpio_connect), (28 bytes).
    Removing drv_fls.o(i.drv_fls_gpio_disconnect), (32 bytes).
    Removing drv_fls.o(i.fls_EnableClk), (12 bytes).
    Removing drv_fls.o(i.fls_busy_pending), (12 bytes).
    Removing drv_fls.o(i.fls_clear_irq_status), (6 bytes).
    Removing drv_fls.o(i.fls_ctrl_cfg_init), (72 bytes).
    Removing drv_fls.o(i.fls_ddat_enable), (24 bytes).
    Removing drv_fls.o(i.fls_de_init), (52 bytes).
    Removing drv_fls.o(i.fls_descr), (10 bytes).
    Removing drv_fls.o(i.fls_disable_it), (36 bytes).
    Removing drv_fls.o(i.fls_en_scr), (10 bytes).
    Removing drv_fls.o(i.fls_enable_it), (48 bytes).
    Removing drv_fls.o(i.fls_get_crcout), (4 bytes).
    Removing drv_fls.o(i.fls_get_default_fls_config), (20 bytes).
    Removing drv_fls.o(i.fls_get_default_spi_config), (44 bytes).
    Removing drv_fls.o(i.fls_get_default_tuning), (12 bytes).
    Removing drv_fls.o(i.fls_get_tuning), (18 bytes).
    Removing drv_fls.o(i.fls_init), (62 bytes).
    Removing drv_fls.o(i.fls_qadr_enable), (22 bytes).
    Removing drv_fls.o(i.fls_qcmd_enable), (22 bytes).
    Removing drv_fls.o(i.fls_qdat_enable), (22 bytes).
    Removing drv_fls.o(i.fls_read_byte_data), (130 bytes).
    Removing drv_fls.o(i.fls_read_cmd), (104 bytes).
    Removing drv_fls.o(i.fls_read_cmd_it), (110 bytes).
    Removing drv_fls.o(i.fls_reset_crc), (18 bytes).
    Removing drv_fls.o(i.fls_scr_clear), (10 bytes).
    Removing drv_fls.o(i.fls_set_addr_dummy), (32 bytes).
    Removing drv_fls.o(i.fls_set_addr_len), (32 bytes).
    Removing drv_fls.o(i.fls_set_mc_irq_mask), (26 bytes).
    Removing drv_fls.o(i.fls_set_read), (10 bytes).
    Removing drv_fls.o(i.fls_set_tuning), (24 bytes).
    Removing drv_fls.o(i.fls_set_write), (10 bytes).
    Removing drv_fls.o(i.fls_single_mode), (16 bytes).
    Removing drv_fls.o(i.fls_spi_init), (180 bytes).
    Removing drv_fls.o(i.fls_spi_start), (10 bytes).
    Removing drv_fls.o(i.fls_swrst), (18 bytes).
    Removing drv_fls.o(i.fls_write_byte_data), (164 bytes).
    Removing drv_fls.o(i.fls_write_cmd), (58 bytes).
    Removing drv_fls.o(.data), (4 bytes).
    Removing drv_gpio.o(.rev16_text), (4 bytes).
    Removing drv_gpio.o(.revsh_text), (4 bytes).
    Removing drv_gpio.o(i.drv_gpio_get_pull_state), (224 bytes).
    Removing drv_gpio.o(i.drv_gpio_register_ap_reset_callback), (12 bytes).
    Removing drv_gpio.o(i.drv_gpio_register_callback), (20 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_driving_strength), (312 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_int), (80 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_schmitt_trigger), (168 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_slew_rate), (168 bytes).
    Removing drv_i2c_dma.o(.rev16_text), (4 bytes).
    Removing drv_i2c_dma.o(.revsh_text), (4 bytes).
    Removing drv_i2c_dma.o(i.drv_i2c_dma_callback), (52 bytes).
    Removing drv_i2c_dma.o(i.drv_i2c_dma_init), (172 bytes).
    Removing drv_i2c_dma.o(i.drv_i2c_enable_rx_dma), (26 bytes).
    Removing drv_i2c_dma.o(i.drv_i2c_enable_tx_dma), (24 bytes).
    Removing drv_i2c_dma.o(i.drv_i2c_master_read_dma), (92 bytes).
    Removing drv_i2c_dma.o(i.drv_i2c_master_write_dma), (60 bytes).
    Removing drv_i2c_dma.o(i.drv_i2c_master_write_read_cmd), (62 bytes).
    Removing drv_i2c_dma.o(i.drv_i2c_set_dma_irq_callback), (88 bytes).
    Removing drv_i2c_dma.o(i.drv_i2c_slave_write_dma), (24 bytes).
    Removing drv_i2c_dma.o(.bss), (320 bytes).
    Removing drv_i2c_dma.o(.data), (8 bytes).
    Removing drv_i2c_master.o(.rev16_text), (4 bytes).
    Removing drv_i2c_master.o(.revsh_text), (4 bytes).
    Removing drv_i2c_master.o(i.__NVIC_ClearPendingIRQ), (24 bytes).
    Removing drv_i2c_master.o(i.drv_i2c1_set_callback), (12 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_bus_init), (36 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_clear_it_pending_bit), (96 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_deinit), (80 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_disable_intr), (16 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_enable), (16 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_enable_intr), (56 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_get_fifo_status), (28 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_read_data), (32 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_set_fifo_threshold), (24 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_set_sys_mask), (48 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_m_write_data), (32 bytes).
    Removing drv_i2c_master.o(i.drv_i2c_master_init), (140 bytes).
    Removing drv_i2c_slave.o(.rev16_text), (4 bytes).
    Removing drv_i2c_slave.o(.revsh_text), (4 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c0_set_callback), (12 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_clear_it_pending_bit), (66 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_config_intr), (4 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_enable), (8 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_get_fifo_status), (20 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_read_data), (30 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_set_fifo_threshold), (16 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_set_intr), (80 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_s_write_data), (28 bytes).
    Removing drv_i2c_slave.o(i.drv_i2c_slave_init), (50 bytes).
    Removing drv_param_init.o(.rev16_text), (4 bytes).
    Removing drv_param_init.o(.revsh_text), (4 bytes).
    Removing drv_param_init.o(i.drv_param_init_set_sclu_filter), (28 bytes).
    Removing drv_pwr.o(.rev16_text), (4 bytes).
    Removing drv_pwr.o(.revsh_text), (4 bytes).
    Removing drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_cp_mode), (32 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_frame_buff_pd), (28 bytes).
    Removing drv_spi_dma.o(.rev16_text), (4 bytes).
    Removing drv_spi_dma.o(.revsh_text), (4 bytes).
    Removing drv_spi_dma.o(i.__NVIC_ClearPendingIRQ), (24 bytes).
    Removing drv_spi_dma.o(i.drv_spi_abort_dma), (108 bytes).
    Removing drv_spi_dma.o(i.drv_spi_dma_callback), (60 bytes).
    Removing drv_spi_dma.o(i.drv_spi_dma_ch6_init), (208 bytes).
    Removing drv_spi_dma.o(i.drv_spi_dma_init), (220 bytes).
    Removing drv_spi_dma.o(i.drv_spi_set_dma_ch6_irq_callback), (48 bytes).
    Removing drv_spi_dma.o(i.drv_spi_set_dma_irq_callback), (88 bytes).
    Removing drv_spi_dma.o(i.drv_spim_dma_read), (96 bytes).
    Removing drv_spi_dma.o(i.drv_spim_dma_write), (60 bytes).
    Removing drv_spi_dma.o(i.drv_spis_dma_write), (72 bytes).
    Removing drv_spi_dma.o(.bss), (480 bytes).
    Removing drv_spi_dma.o(.data), (16 bytes).
    Removing drv_spi_master.o(.rev16_text), (4 bytes).
    Removing drv_spi_master.o(.revsh_text), (4 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_deinit), (40 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_disable_int), (68 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_enable_int), (72 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_enable_rx_dma), (32 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_enable_tx_dma), (28 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_get_dma_address), (8 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_gpio_init), (32 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_read_data), (32 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_set_intr_callback), (12 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_switch_sclk), (28 bytes).
    Removing drv_spi_master.o(i.drv_spi_m_write_data), (44 bytes).
    Removing drv_spi_master.o(i.drv_spi_master_init), (164 bytes).
    Removing drv_sys_cfg.o(.rev16_text), (4 bytes).
    Removing drv_sys_cfg.o(.revsh_text), (4 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_dma_req_mask), (32 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_read_version0_id), (12 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig), (28 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group), (36 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig), (36 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_set_ap_reset), (28 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_set_dma_rx_req), (16 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_set_dma_tx_req), (16 bytes).
    Removing hal_internal_soft_sync.o(.rev16_text), (4 bytes).
    Removing hal_internal_soft_sync.o(.revsh_text), (4 bytes).
    Removing hal_internal_soft_sync.o(i.hal_intl_svs_deinit_rx), (48 bytes).
    Removing hal_internal_soft_sync.o(i.hal_intl_svs_set_input_frate), (120 bytes).
    Removing drv_dsi_rx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_rx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate), (66 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_version), (4 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_phy_resistor_calibration), (236 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg), (32 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg), (48 bytes).
    Removing drv_dsi_rx.o(i.drv_rx_phy_test_read), (12 bytes).
    Removing drv_dsi_tx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_tx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_force_interrupt), (8 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_get_phy_status), (6 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_forcepll), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_resistor_calibration), (232 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_start), (18 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock), (10 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot), (62 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger), (92 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter), (344 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit), (276 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_sdf_3d), (28 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_bta), (22 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_vpg), (70 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_version), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_vid_shadow), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_read), (10 bytes).
    Removing drv_lcdc.o(.rev16_text), (4 bytes).
    Removing drv_lcdc.o(.revsh_text), (4 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_config_rgb_to_pentile), (6 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_enable), (42 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_update_shadow_reg), (12 bytes).
    Removing drv_memc.o(.rev16_text), (4 bytes).
    Removing drv_memc.o(.revsh_text), (4 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_frm_time), (14 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_int_frame), (28 bytes).
    Removing drv_memc.o(i.drv_memc_set_fb_remaining_line_trigger), (12 bytes).
    Removing drv_memc.o(i.drv_memc_set_read_trigger_line), (16 bytes).
    Removing drv_memc.o(i.drv_memc_set_te_ind), (16 bytes).
    Removing drv_memc.o(i.drv_memc_set_tear_hwclr), (16 bytes).
    Removing drv_memc.o(i.drv_memc_set_vidc_fb_arb), (14 bytes).
    Removing drv_memc.o(i.drv_memc_set_write_trigger_line), (16 bytes).
    Removing drv_rxbr.o(.rev16_text), (4 bytes).
    Removing drv_rxbr.o(.revsh_text), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_dsc_flush), (16 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_cur_hline_rcv_cnt), (8 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_ipi_vsync_interval), (8 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_pix_fmt), (8 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_cmd_filter), (204 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_col_addr), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_compress), (24 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_page_addr), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_soft_reset), (98 bytes).
    Removing drv_vidc.o(.rev16_text), (4 bytes).
    Removing drv_vidc.o(.revsh_text), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_clear_status0), (14 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_cap_pixel), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_signal_frame), (30 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_int_source), (38 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status0), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status1), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status2), (6 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_dsc_thresh), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_frmst_latency), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_inff_thresh), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_irq_line), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_module_enable), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_outff_thresh), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_update_src_format), (14 bytes).
    Removing irq_redirect .o(.rev16_text), (4 bytes).
    Removing irq_redirect .o(.revsh_text), (4 bytes).
    Removing drv_efuse.o(.rev16_text), (4 bytes).
    Removing drv_efuse.o(.revsh_text), (4 bytes).
    Removing drv_efuse.o(i.drv_efuse_crc_cal), (128 bytes).
    Removing drv_efuse.o(i.drv_efuse_get_default_config), (26 bytes).
    Removing drv_efuse.o(i.drv_efuse_int_disable), (12 bytes).
    Removing drv_efuse.o(i.drv_efuse_write), (46 bytes).
    Removing drv_efuse.o(i.drv_efuse_write_req), (22 bytes).
    Removing drv_phy_common.o(.rev16_text), (4 bytes).
    Removing drv_phy_common.o(.revsh_text), (4 bytes).
    Removing drv_phy_common.o(i.drv_phy_test_read), (8 bytes).
    Removing drv_chip_info.o(.rev16_text), (4 bytes).
    Removing drv_chip_info.o(.revsh_text), (4 bytes).
    Removing drv_dsc_dec.o(.rev16_text), (4 bytes).
    Removing drv_dsc_dec.o(.revsh_text), (4 bytes).
    Removing drv_dsc_dec.o(i.drv_dsc_dec_set_u32_pps), (120 bytes).
    Removing hal_spi_slave.o(.rev16_text), (4 bytes).
    Removing hal_spi_slave.o(.revsh_text), (4 bytes).
    Removing hal_spi_slave.o(i.hal_spi_s_set_high_impedance), (100 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_auto_transfer_abort), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_auto_transfer_start), (56 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_busy), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_deinit), (10 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_disable), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_enable), (96 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_flush_fifo), (20 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_get_rxfifo_notempty), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_gpio_init), (8 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_init), (76 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_read_data), (10 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_register_callback), (12 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_reset_tx), (68 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_set_auto_rx_buffer), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_set_auto_tx_buffer), (16 bytes).
    Removing hal_spi_slave.o(i.hal_spi_slave_write_data), (14 bytes).
    Removing norflash.o(.rev16_text), (4 bytes).
    Removing norflash.o(.revsh_text), (4 bytes).
    Removing norflash.o(i.norflash_best_cfg_init), (44 bytes).
    Removing norflash.o(i.norflash_big_end_clear), (14 bytes).
    Removing norflash.o(i.norflash_big_end_enable), (20 bytes).
    Removing norflash.o(i.norflash_check_crc32), (14 bytes).
    Removing norflash.o(i.norflash_check_id), (72 bytes).
    Removing norflash.o(i.norflash_dma_callback), (24 bytes).
    Removing norflash.o(i.norflash_dma_read), (156 bytes).
    Removing norflash.o(i.norflash_dma_write), (252 bytes).
    Removing norflash.o(i.norflash_dual_read), (60 bytes).
    Removing norflash.o(i.norflash_dual_write), (112 bytes).
    Removing norflash.o(i.norflash_en4b), (40 bytes).
    Removing norflash.o(i.norflash_en_quad), (116 bytes).
    Removing norflash.o(i.norflash_en_quad_check), (64 bytes).
    Removing norflash.o(i.norflash_erase_block), (44 bytes).
    Removing norflash.o(i.norflash_erase_chip), (28 bytes).
    Removing norflash.o(i.norflash_erase_sector), (44 bytes).
    Removing norflash.o(i.norflash_ex4b), (40 bytes).
    Removing norflash.o(i.norflash_exit_quad), (76 bytes).
    Removing norflash.o(i.norflash_get_dual_hstatus), (52 bytes).
    Removing norflash.o(i.norflash_get_hstatus), (52 bytes).
    Removing norflash.o(i.norflash_get_status), (52 bytes).
    Removing norflash.o(i.norflash_init), (48 bytes).
    Removing norflash.o(i.norflash_quad_read), (76 bytes).
    Removing norflash.o(i.norflash_quad_write), (108 bytes).
    Removing norflash.o(i.norflash_read), (28 bytes).
    Removing norflash.o(i.norflash_read_config_reg), (36 bytes).
    Removing norflash.o(i.norflash_read_id), (20 bytes).
    Removing norflash.o(i.norflash_read_uid), (52 bytes).
    Removing norflash.o(i.norflash_reset), (2 bytes).
    Removing norflash.o(i.norflash_reset_crc32), (32 bytes).
    Removing norflash.o(i.norflash_set_best_cfg), (50 bytes).
    Removing norflash.o(i.norflash_set_best_read_cfg), (84 bytes).
    Removing norflash.o(i.norflash_set_best_write_cfg), (84 bytes).
    Removing norflash.o(i.norflash_switch_fls_spi), (112 bytes).
    Removing norflash.o(i.norflash_write), (96 bytes).
    Removing norflash.o(i.norflash_write_disable), (64 bytes).
    Removing norflash.o(i.norflash_write_enable), (56 bytes).
    Removing norflash.o(i.norflash_write_endian_scr), (132 bytes).
    Removing norflash.o(.bss), (412 bytes).
    Removing norflash.o(.bss), (32 bytes).
    Removing norflash.o(.data), (2 bytes).
    Removing drv_fls_dma.o(.rev16_text), (4 bytes).
    Removing drv_fls_dma.o(.revsh_text), (4 bytes).
    Removing drv_fls_dma.o(i.fls_abort_dma), (42 bytes).
    Removing drv_fls_dma.o(i.fls_dma_disable), (10 bytes).
    Removing drv_fls_dma.o(i.fls_dma_enable), (10 bytes).
    Removing drv_fls_dma.o(i.fls_dma_read_prepare), (86 bytes).
    Removing drv_fls_dma.o(i.fls_dma_write_prepare), (82 bytes).
    Removing drv_fls_dma.o(i.fls_read_dmacallback), (32 bytes).
    Removing drv_fls_dma.o(i.fls_transfer_create_handle_dma), (208 bytes).
    Removing drv_fls_dma.o(i.fls_transfer_dma), (112 bytes).
    Removing drv_fls_dma.o(i.fls_transfer_get_receive_count_dma), (44 bytes).
    Removing drv_fls_dma.o(i.fls_write_dmacallback), (32 bytes).
    Removing drv_fls_dma.o(.data), (8 bytes).
    Removing drv_pwm.o(.rev16_text), (4 bytes).
    Removing drv_pwm.o(.revsh_text), (4 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_clear_pwm_int_all), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_enable), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_counter_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_current_count), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_high_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_get_low_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_register_callback), (24 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_set_pwm_int), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_in_set_sys_int), (64 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_enable), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_get_sync_flag), (16 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_pause), (28 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_control), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_period), (12 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_sync_mode), (32 bytes).
    Removing drv_pwm.o(i.drv_pwm_out_set_threshold), (12 bytes).
    Removing drv_spi_slave.o(.rev16_text), (4 bytes).
    Removing drv_spi_slave.o(.revsh_text), (4 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_deinit), (40 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_disable_int), (68 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_enable_int), (72 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_enable_rx_dma), (32 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_enable_tx_dma), (28 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_get_dma_address), (8 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_gpio_init), (24 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_read_data), (32 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_switch_sclk), (28 bytes).
    Removing drv_spi_slave.o(i.drv_spi_s_write_data), (44 bytes).
    Removing drv_spi_slave.o(i.drv_spi_slave_init), (76 bytes).
    Removing drv_swire.o(.rev16_text), (4 bytes).
    Removing drv_swire.o(.revsh_text), (4 bytes).
    Removing drv_swire.o(i.drv_swire_enable), (28 bytes).
    Removing drv_swire.o(i.drv_swire_register_callback), (12 bytes).
    Removing drv_swire.o(i.drv_swire_set_bit_time), (24 bytes).
    Removing drv_swire.o(i.drv_swire_set_power_down), (28 bytes).
    Removing drv_swire.o(i.drv_swire_set_pulse_count), (12 bytes).
    Removing drv_timer.o(.rev16_text), (4 bytes).
    Removing drv_timer.o(.revsh_text), (4 bytes).
    Removing drv_timer.o(i.drv_timer_get_prescaler), (16 bytes).
    Removing drv_timer.o(i.drv_timer_get_status), (38 bytes).
    Removing drv_timer.o(i.drv_timer_register_callback), (20 bytes).
    Removing drv_timer.o(i.drv_timer_set_prescaler), (40 bytes).
    Removing drv_timer.o(i.drv_timer_set_repeat), (16 bytes).
    Removing drv_uart.o(.rev16_text), (4 bytes).
    Removing drv_uart.o(.revsh_text), (4 bytes).
    Removing drv_uart.o(i.UART_AbortReceive), (30 bytes).
    Removing drv_uart.o(i.UART_AbortSend), (30 bytes).
    Removing drv_uart.o(i.UART_Deinit), (28 bytes).
    Removing drv_uart.o(i.UART_Disable_IT), (68 bytes).
    Removing drv_uart.o(i.UART_EnableDma), (32 bytes).
    Removing drv_uart.o(i.UART_Enable_IT), (44 bytes).
    Removing drv_uart.o(i.UART_GetDefaultConfig), (72 bytes).
    Removing drv_uart.o(i.UART_GetFIFO_Ctrl), (20 bytes).
    Removing drv_uart.o(i.UART_GetReceiveCount), (22 bytes).
    Removing drv_uart.o(i.UART_GetReceiveStatus), (20 bytes).
    Removing drv_uart.o(i.UART_GetRxRingBufferLength), (28 bytes).
    Removing drv_uart.o(i.UART_GetSendCount), (22 bytes).
    Removing drv_uart.o(i.UART_GetSendStatus), (20 bytes).
    Removing drv_uart.o(i.UART_ReadBlocking), (32 bytes).
    Removing drv_uart.o(i.UART_ReceiveNonBlocking), (50 bytes).
    Removing drv_uart.o(i.UART_ResetTxFIFO), (36 bytes).
    Removing drv_uart.o(i.UART_SendNonBlocking), (38 bytes).
    Removing drv_uart.o(i.UART_TransferCreateHandle), (96 bytes).
    Removing drv_uart.o(i.UART_TransferStartRingBuffer), (30 bytes).
    Removing drv_uart.o(.constdata), (1 bytes).
    Removing drv_uart_dma.o(.rev16_text), (4 bytes).
    Removing drv_uart_dma.o(.revsh_text), (4 bytes).
    Removing drv_uart_dma.o(i.UART_DMAInit), (76 bytes).
    Removing drv_uart_dma.o(i.UART_TransferAbortReceiveDMA), (16 bytes).
    Removing drv_uart_dma.o(i.UART_TransferAbortSendDMA), (16 bytes).
    Removing drv_uart_dma.o(i.UART_TransferCreateHandleDMA), (176 bytes).
    Removing drv_uart_dma.o(i.UART_TransferGetReceiveCountDMA), (44 bytes).
    Removing drv_uart_dma.o(i.UART_TransferReceiveDMA), (68 bytes).
    Removing drv_uart_dma.o(i.UART_TransferReceiveDMACallback), (34 bytes).
    Removing drv_uart_dma.o(i.UART_TransferSendDMA), (68 bytes).
    Removing drv_uart_dma.o(i.UART_TransferSendDMACallback), (34 bytes).
    Removing drv_uart_dma.o(.data), (8 bytes).
    Removing drv_wdg.o(.rev16_text), (4 bytes).
    Removing drv_wdg.o(.revsh_text), (4 bytes).
    Removing drv_wdg.o(i.drv_wdg_enable), (32 bytes).
    Removing drv_wdg.o(i.drv_wdg_load_match), (12 bytes).
    Removing drv_wdg.o(i.drv_wdg_register_callback), (12 bytes).
    Removing drv_wdg.o(i.drv_wdg_sel_mode), (28 bytes).
    Removing drv_wdg.o(i.drv_wdg_set_repeat), (12 bytes).
    Removing dcs_packet_fifo.o(i.dcs_packet_get_fifo_size), (16 bytes).
    Removing dflti.o(.text), (40 bytes).

706 unused section(s) (total 42697 bytes) removed from the image.

==============================================================================

Image Symbol Table

    Local Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    ../clib/../cmprslib/zerorunl2.c          0x00000000   Number         0  __dczerorl2.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uldiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uidiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  idiv.o ABSOLUTE
    ../clib/microlib/errno.c                 0x00000000   Number         0  errno.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry5.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry2.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11a.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llshl.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llushr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llsshr.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfa.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf5.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf6.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf7.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf8.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf4.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf3.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfb.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf0.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf1.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf2.o ABSOLUTE
    ../clib/microlib/printf/stubs.s          0x00000000   Number         0  stubs.o ABSOLUTE
    ../clib/microlib/stdio/streams.c         0x00000000   Number         0  stdout.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpya.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpyb.o ABSOLUTE
    ../clib/microlib/string/memset.c         0x00000000   Number         0  memseta.o ABSOLUTE
    ../clib/microlib/stubs.s                 0x00000000   Number         0  iusefp.o ABSOLUTE
    ../fplib/microlib/f2d.c                  0x00000000   Number         0  f2d.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  fadd.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  dadd.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  ddiv.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  fdiv.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  fepilogue.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  depilogue.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixul.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixui.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixi.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  ffixui.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  ffixi.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  fflti.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  dflti.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  ffltui.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  dfltui.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  fmul.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  dmul.o ABSOLUTE
    ../fplib/microlib/fpscalb.c              0x00000000   Number         0  fscalb.o ABSOLUTE
    ../fplib/microlib/fpsqrt.c               0x00000000   Number         0  dsqrt.o ABSOLUTE
    ../mathlib/ceil.c                        0x00000000   Number         0  ceil.o ABSOLUTE
    ../mathlib/sqrt.c                        0x00000000   Number         0  sqrt.o ABSOLUTE
    ../mathlib/sqrt.c                        0x00000000   Number         0  sqrt_x.o ABSOLUTE
    ..\..\..\src\common\tau_delay.c          0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\..\..\src\common\tau_log.c            0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\..\..\src\driver\robin\src\drv_chip_info.c 0x00000000   Number         0  drv_chip_info.o ABSOLUTE
    ..\..\..\src\driver\robin\src\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\..\..\src\driver\source\robin\drv\irq_redirect .c 0x00000000   Number         0  irq_redirect .o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\internal\dcs_packet_fifo.c 0x00000000   Number         0  dcs_packet_fifo.o ABSOLUTE
    ..\..\..\src\driver\source\robin\hal\internal\hal_internal_soft_sync.c 0x00000000   Number         0  hal_internal_soft_sync.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_fls.c 0x00000000   Number         0  drv_fls.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_fls_dma.c 0x00000000   Number         0  drv_fls_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_i2c_dma.c 0x00000000   Number         0  drv_i2c_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_i2c_master.c 0x00000000   Number         0  drv_i2c_master.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_i2c_slave.c 0x00000000   Number         0  drv_i2c_slave.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_param_init.c 0x00000000   Number         0  drv_param_init.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_pwm.c 0x00000000   Number         0  drv_pwm.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_spi_dma.c 0x00000000   Number         0  drv_spi_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_spi_master.c 0x00000000   Number         0  drv_spi_master.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_spi_slave.c 0x00000000   Number         0  drv_spi_slave.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_uart_dma.c 0x00000000   Number         0  drv_uart_dma.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\drv\drv_wdg.c 0x00000000   Number         0  drv_wdg.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_i2c_master.c 0x00000000   Number         0  hal_i2c_master.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_i2c_slave.c 0x00000000   Number         0  hal_i2c_slave.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_spi_master.c 0x00000000   Number         0  hal_spi_master.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_spi_slave.c 0x00000000   Number         0  hal_spi_slave.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\internal\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\..\..\src\sdk\robin\src\hal\internal\norflash.c 0x00000000   Number         0  norflash.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_delay.c     0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_log.c       0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\\..\\..\\src\\driver\\robin\\src\\drv_chip_info.c 0x00000000   Number         0  drv_chip_info.o ABSOLUTE
    ..\\..\\..\\src\\driver\\robin\\src\\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\drv\\irq_redirect .c 0x00000000   Number         0  irq_redirect .o ABSOLUTE
    ..\\..\\..\\src\\driver\\source\\robin\\hal\\internal\\hal_internal_soft_sync.c 0x00000000   Number         0  hal_internal_soft_sync.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_fls.c 0x00000000   Number         0  drv_fls.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_fls_dma.c 0x00000000   Number         0  drv_fls_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_i2c_dma.c 0x00000000   Number         0  drv_i2c_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_i2c_master.c 0x00000000   Number         0  drv_i2c_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_i2c_slave.c 0x00000000   Number         0  drv_i2c_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_param_init.c 0x00000000   Number         0  drv_param_init.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_pwm.c 0x00000000   Number         0  drv_pwm.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_spi_dma.c 0x00000000   Number         0  drv_spi_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_spi_master.c 0x00000000   Number         0  drv_spi_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_spi_slave.c 0x00000000   Number         0  drv_spi_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_uart_dma.c 0x00000000   Number         0  drv_uart_dma.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\drv\\drv_wdg.c 0x00000000   Number         0  drv_wdg.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_i2c_master.c 0x00000000   Number         0  hal_i2c_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_i2c_slave.c 0x00000000   Number         0  hal_i2c_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_spi_master.c 0x00000000   Number         0  hal_spi_master.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_spi_slave.c 0x00000000   Number         0  hal_spi_slave.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\internal\\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\\..\\..\\src\\sdk\\robin\\src\\hal\\internal\\norflash.c 0x00000000   Number         0  norflash.o ABSOLUTE
    ..\\src\\app\\demo\\ap_demo.c            0x00000000   Number         0  ap_demo.o ABSOLUTE
    ..\\src\\app\\demo\\app_tp_for_custom_s8.c 0x00000000   Number         0  app_tp_for_custom_s8.o ABSOLUTE
    ..\\src\\app\\demo\\app_tp_st_touch.c    0x00000000   Number         0  app_tp_st_touch.o ABSOLUTE
    ..\\src\\app\\demo\\app_tp_transfer.c    0x00000000   Number         0  app_tp_transfer.o ABSOLUTE
    ..\\src\\app\\main.c                     0x00000000   Number         0  main.o ABSOLUTE
    ..\\src\\board\\board.c                  0x00000000   Number         0  board.o ABSOLUTE
    ..\src\app\demo\ap_demo.c                0x00000000   Number         0  ap_demo.o ABSOLUTE
    ..\src\app\demo\app_tp_for_custom_s8.c   0x00000000   Number         0  app_tp_for_custom_s8.o ABSOLUTE
    ..\src\app\demo\app_tp_st_touch.c        0x00000000   Number         0  app_tp_st_touch.o ABSOLUTE
    ..\src\app\demo\app_tp_transfer.c        0x00000000   Number         0  app_tp_transfer.o ABSOLUTE
    ..\src\app\main.c                        0x00000000   Number         0  main.o ABSOLUTE
    ..\src\board\board.c                     0x00000000   Number         0  board.o ABSOLUTE
    ..\src\board\startup\startup_ARMCM0.s    0x00000000   Number         0  startup_armcm0.o ABSOLUTE
    cdcmple.s                                0x00000000   Number         0  cdcmple.o ABSOLUTE
    cdrcmple.s                               0x00000000   Number         0  cdrcmple.o ABSOLUTE
    cfcmple.s                                0x00000000   Number         0  cfcmple.o ABSOLUTE
    cfrcmple.s                               0x00000000   Number         0  cfrcmple.o ABSOLUTE
    dc.s                                     0x00000000   Number         0  dc.o ABSOLUTE
    handlers.s                               0x00000000   Number         0  handlers.o ABSOLUTE
    init.s                                   0x00000000   Number         0  init.o ABSOLUTE
    RESET                                    0x00010000   Section      192  startup_armcm0.o(RESET)
    .ARM.Collect$$$$00000000                 0x000100c0   Section        0  entry.o(.ARM.Collect$$$$00000000)
    .ARM.Collect$$$$00000001                 0x000100c0   Section        4  entry2.o(.ARM.Collect$$$$00000001)
    .ARM.Collect$$$$00000004                 0x000100c4   Section        4  entry5.o(.ARM.Collect$$$$00000004)
    .ARM.Collect$$$$00000008                 0x000100c8   Section        0  entry7b.o(.ARM.Collect$$$$00000008)
    .ARM.Collect$$$$0000000A                 0x000100c8   Section        0  entry8b.o(.ARM.Collect$$$$0000000A)
    .ARM.Collect$$$$0000000B                 0x000100c8   Section        8  entry9a.o(.ARM.Collect$$$$0000000B)
    .ARM.Collect$$$$0000000D                 0x000100d0   Section        0  entry10a.o(.ARM.Collect$$$$0000000D)
    .ARM.Collect$$$$0000000F                 0x000100d0   Section        0  entry11a.o(.ARM.Collect$$$$0000000F)
    .ARM.Collect$$$$00002712                 0x000100d0   Section        4  entry2.o(.ARM.Collect$$$$00002712)
    __lit__00000000                          0x000100d0   Data           4  entry2.o(.ARM.Collect$$$$00002712)
    .text                                    0x000100d4   Section      120  startup_armcm0.o(.text)
    .text                                    0x0001014c   Section        0  uidiv.o(.text)
    .text                                    0x00010178   Section        0  idiv.o(.text)
    .text                                    0x000101a0   Section        0  memcpya.o(.text)
    .text                                    0x000101c4   Section        0  memseta.o(.text)
    .text                                    0x000101e8   Section        0  fadd.o(.text)
    .text                                    0x0001029a   Section        0  fmul.o(.text)
    .text                                    0x00010314   Section        0  fdiv.o(.text)
    .text                                    0x00010390   Section        0  fscalb.o(.text)
    .text                                    0x000103a8   Section        0  dadd.o(.text)
    .text                                    0x0001050c   Section        0  dmul.o(.text)
    .text                                    0x000105dc   Section        0  ddiv.o(.text)
    .text                                    0x000106cc   Section        0  fflti.o(.text)
    .text                                    0x000106e2   Section        0  ffltui.o(.text)
    .text                                    0x000106f0   Section        0  dfltui.o(.text)
    .text                                    0x0001070c   Section        0  ffixi.o(.text)
    .text                                    0x0001073e   Section        0  ffixui.o(.text)
    .text                                    0x00010768   Section        0  dfixi.o(.text)
    .text                                    0x000107b0   Section        0  dfixui.o(.text)
    .text                                    0x000107ec   Section        0  f2d.o(.text)
    .text                                    0x00010814   Section       40  cdcmple.o(.text)
    .text                                    0x0001083c   Section       20  cfcmple.o(.text)
    .text                                    0x00010850   Section       20  cfrcmple.o(.text)
    .text                                    0x00010864   Section        0  uldiv.o(.text)
    .text                                    0x000108c4   Section        0  llshl.o(.text)
    .text                                    0x000108e4   Section        0  llushr.o(.text)
    .text                                    0x00010906   Section        0  llsshr.o(.text)
    .text                                    0x0001092c   Section        0  iusefp.o(.text)
    .text                                    0x0001092c   Section        0  fepilogue.o(.text)
    .text                                    0x000109ae   Section        0  depilogue.o(.text)
    .text                                    0x00010a6c   Section        0  dsqrt.o(.text)
    .text                                    0x00010b10   Section        0  dfixul.o(.text)
    .text                                    0x00010b50   Section       40  cdrcmple.o(.text)
    .text                                    0x00010b78   Section       36  init.o(.text)
    .text                                    0x00010b9c   Section        0  __dczerorl2.o(.text)
    i.ADC_IRQn_Handler                       0x00010bf4   Section        0  irq_redirect .o(i.ADC_IRQn_Handler)
    i.AP_NRESET_IRQn_Handler                 0x00010c0c   Section        0  irq_redirect .o(i.AP_NRESET_IRQn_Handler)
    i.DMA_IRQn_Handler                       0x00010c24   Section        0  irq_redirect .o(i.DMA_IRQn_Handler)
    i.EXTI_INT0_IRQn_Handler                 0x00010c38   Section        0  irq_redirect .o(i.EXTI_INT0_IRQn_Handler)
    i.EXTI_INT1_IRQn_Handler                 0x00010c54   Section        0  irq_redirect .o(i.EXTI_INT1_IRQn_Handler)
    i.EXTI_INT2_IRQn_Handler                 0x00010c70   Section        0  irq_redirect .o(i.EXTI_INT2_IRQn_Handler)
    i.EXTI_INT3_IRQn_Handler                 0x00010c8c   Section        0  irq_redirect .o(i.EXTI_INT3_IRQn_Handler)
    i.EXTI_INT4_IRQn_Handler                 0x00010ca8   Section        0  irq_redirect .o(i.EXTI_INT4_IRQn_Handler)
    i.EXTI_INT5_IRQn_Handler                 0x00010cc4   Section        0  irq_redirect .o(i.EXTI_INT5_IRQn_Handler)
    i.EXTI_INT6_IRQn_Handler                 0x00010ce0   Section        0  irq_redirect .o(i.EXTI_INT6_IRQn_Handler)
    i.EXTI_INT7_IRQn_Handler                 0x00010cfc   Section        0  irq_redirect .o(i.EXTI_INT7_IRQn_Handler)
    i.FLSCTRL_IRQn_Handler                   0x00010d18   Section        0  irq_redirect .o(i.FLSCTRL_IRQn_Handler)
    i.Gpio_swire_output                      0x00010d2c   Section        0  ap_demo.o(i.Gpio_swire_output)
    i.HardFault_Handler                      0x00010d7c   Section        0  irq_redirect .o(i.HardFault_Handler)
    i.I2C0_IRQn_Handler                      0x00010d90   Section        0  irq_redirect .o(i.I2C0_IRQn_Handler)
    i.I2C1_IRQn_Handler                      0x00010da8   Section        0  irq_redirect .o(i.I2C1_IRQn_Handler)
    i.LCDC_IRQn_Handler                      0x00010dc0   Section        0  irq_redirect .o(i.LCDC_IRQn_Handler)
    i.LOG_printf                             0x00010dd8   Section        0  tau_log.o(i.LOG_printf)
    i.MEMC_IRQn_Handler                      0x00010e00   Section        0  irq_redirect .o(i.MEMC_IRQn_Handler)
    i.MIPI_RX_IRQn_Handler                   0x00010e18   Section        0  irq_redirect .o(i.MIPI_RX_IRQn_Handler)
    i.MIPI_TX_IRQn_Handler                   0x00010e30   Section        0  irq_redirect .o(i.MIPI_TX_IRQn_Handler)
    i.PWMDET_IRQn_Handler                    0x00010e48   Section        0  irq_redirect .o(i.PWMDET_IRQn_Handler)
    i.PhoneDisOffDeal                        0x00010e64   Section        0  ap_demo.o(i.PhoneDisOffDeal)
    PhoneDisOffDeal                          0x00010e65   Thumb Code   162  ap_demo.o(i.PhoneDisOffDeal)
    i.SPIM_IRQn_Handler                      0x00010f28   Section        0  irq_redirect .o(i.SPIM_IRQn_Handler)
    i.SPIS_IRQn_Handler                      0x00010f44   Section        0  irq_redirect .o(i.SPIS_IRQn_Handler)
    i.SWIRE_IRQn_Handler                     0x00010f60   Section        0  irq_redirect .o(i.SWIRE_IRQn_Handler)
    i.SysTick_Handler                        0x00010f7c   Section        0  irq_redirect .o(i.SysTick_Handler)
    i.TIMER0_IRQn_Handler                    0x00010f94   Section        0  irq_redirect .o(i.TIMER0_IRQn_Handler)
    i.TIMER1_IRQn_Handler                    0x00010fac   Section        0  irq_redirect .o(i.TIMER1_IRQn_Handler)
    i.TIMER2_IRQn_Handler                    0x00010fc4   Section        0  irq_redirect .o(i.TIMER2_IRQn_Handler)
    i.TIMER3_IRQn_Handler                    0x00010fdc   Section        0  irq_redirect .o(i.TIMER3_IRQn_Handler)
    i.UART_DisableDma                        0x00010ff4   Section        0  drv_uart.o(i.UART_DisableDma)
    i.UART_GetInstance                       0x00010ff6   Section        0  drv_uart.o(i.UART_GetInstance)
    i.__scatterload_null                     0x00010ffa   Section        2  handlers.o(i.__scatterload_null)
    i.drv_dsi_rx_set_inten                   0x00010ffc   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    .ARM.__at_0x11000                        0x00011000   Section       20  drv_common.o(.ARM.__at_0x11000)
    i.drv_dsi_tx_command_put_payload         0x00011014   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    .ARM.__at_0x11018                        0x00011018   Section        4  drv_common.o(.ARM.__at_0x11018)
    i.UART0_IRQ_Handle                       0x0001101c   Section        0  drv_uart.o(i.UART0_IRQ_Handle)
    i.UART_IRQn_Handler                      0x00011038   Section        0  irq_redirect .o(i.UART_IRQn_Handler)
    i.UART_ResetRxFIFO                       0x00011050   Section        0  drv_uart.o(i.UART_ResetRxFIFO)
    i.UART_SetBaudRate                       0x00011074   Section        0  drv_uart.o(i.UART_SetBaudRate)
    i.UART_SwitchSCLK                        0x000110bc   Section        0  drv_uart.o(i.UART_SwitchSCLK)
    i.UART_TransferHandleIRQ                 0x000110d6   Section        0  drv_uart.o(i.UART_TransferHandleIRQ)
    i.UART_WriteBlocking                     0x0001120a   Section        0  drv_uart.o(i.UART_WriteBlocking)
    i.UART_init                              0x00011224   Section        0  drv_uart.o(i.UART_init)
    i.VIDC_IRQn_Handler                      0x000112e0   Section        0  irq_redirect .o(i.VIDC_IRQn_Handler)
    i.VPRE_IRQn_Handler                      0x000112f8   Section        0  irq_redirect .o(i.VPRE_IRQn_Handler)
    i.WDG_IRQn_Handler                       0x00011310   Section        0  irq_redirect .o(i.WDG_IRQn_Handler)
    i.__0printf                              0x00011328   Section        0  printfa.o(i.__0printf)
    i.__0vsprintf                            0x00011348   Section        0  printfa.o(i.__0vsprintf)
    i.__ARM_clz                              0x0001136c   Section        0  depilogue.o(i.__ARM_clz)
    i.__ARM_common_switch8                   0x0001139a   Section        0  hal_dsi_rx_ctrl.o(i.__ARM_common_switch8)
    i.__NVIC_ClearPendingIRQ                 0x000113b4   Section        0  drv_spi_master.o(i.__NVIC_ClearPendingIRQ)
    __NVIC_ClearPendingIRQ                   0x000113b5   Thumb Code    18  drv_spi_master.o(i.__NVIC_ClearPendingIRQ)
    i.__NVIC_DisableIRQ                      0x000113cc   Section        0  drv_rxbr.o(i.__NVIC_DisableIRQ)
    __NVIC_DisableIRQ                        0x000113cd   Thumb Code    26  drv_rxbr.o(i.__NVIC_DisableIRQ)
    i.__NVIC_EnableIRQ                       0x000113ec   Section        0  drv_rxbr.o(i.__NVIC_EnableIRQ)
    __NVIC_EnableIRQ                         0x000113ed   Thumb Code    18  drv_rxbr.o(i.__NVIC_EnableIRQ)
    i.__NVIC_SetPriority                     0x00011404   Section        0  hal_spi_slave.o(i.__NVIC_SetPriority)
    __NVIC_SetPriority                       0x00011405   Thumb Code    60  hal_spi_slave.o(i.__NVIC_SetPriority)
    i.__scatterload_copy                     0x00011448   Section       14  handlers.o(i.__scatterload_copy)
    i.__scatterload_zeroinit                 0x00011456   Section       14  handlers.o(i.__scatterload_zeroinit)
    i.__set_errno                            0x00011464   Section        0  errno.o(i.__set_errno)
    i._fp_digits                             0x00011470   Section        0  printfa.o(i._fp_digits)
    _fp_digits                               0x00011471   Thumb Code   344  printfa.o(i._fp_digits)
    i._printf_core                           0x000115e4   Section        0  printfa.o(i._printf_core)
    _printf_core                             0x000115e5   Thumb Code  1754  printfa.o(i._printf_core)
    i._printf_post_padding                   0x00011cd0   Section        0  printfa.o(i._printf_post_padding)
    _printf_post_padding                     0x00011cd1   Thumb Code    32  printfa.o(i._printf_post_padding)
    i._printf_pre_padding                    0x00011cf0   Section        0  printfa.o(i._printf_pre_padding)
    _printf_pre_padding                      0x00011cf1   Thumb Code    44  printfa.o(i._printf_pre_padding)
    i._sputc                                 0x00011d1c   Section        0  printfa.o(i._sputc)
    _sputc                                   0x00011d1d   Thumb Code    10  printfa.o(i._sputc)
    i.ap_dcs_read                            0x00011d28   Section        0  ap_demo.o(i.ap_dcs_read)
    ap_dcs_read                              0x00011d29   Thumb Code  4158  ap_demo.o(i.ap_dcs_read)
    i.ap_demo                                0x00012da0   Section        0  ap_demo.o(i.ap_demo)
    i.ap_get_reg_df                          0x00012ec4   Section        0  ap_demo.o(i.ap_get_reg_df)
    ap_get_reg_df                            0x00012ec5   Thumb Code    68  ap_demo.o(i.ap_get_reg_df)
    i.ap_get_tp_calibration_status_01        0x00012f10   Section        0  app_tp_st_touch.o(i.ap_get_tp_calibration_status_01)
    i.ap_set_backlight_51                    0x00012f30   Section        0  ap_demo.o(i.ap_set_backlight_51)
    ap_set_backlight_51                      0x00012f31   Thumb Code    78  ap_demo.o(i.ap_set_backlight_51)
    i.ap_set_display_off                     0x00012fa4   Section        0  ap_demo.o(i.ap_set_display_off)
    ap_set_display_off                       0x00012fa5   Thumb Code    30  ap_demo.o(i.ap_set_display_off)
    i.ap_set_display_on                      0x00012fe8   Section        0  ap_demo.o(i.ap_set_display_on)
    ap_set_display_on                        0x00012fe9   Thumb Code    16  ap_demo.o(i.ap_set_display_on)
    i.ap_set_enter_sleep_mode                0x00013020   Section        0  ap_demo.o(i.ap_set_enter_sleep_mode)
    ap_set_enter_sleep_mode                  0x00013021   Thumb Code    74  ap_demo.o(i.ap_set_enter_sleep_mode)
    i.ap_set_exit_sleep_mode                 0x000130a0   Section        0  ap_demo.o(i.ap_set_exit_sleep_mode)
    ap_set_exit_sleep_mode                   0x000130a1   Thumb Code    58  ap_demo.o(i.ap_set_exit_sleep_mode)
    i.ap_set_hbm_53                          0x00013110   Section        0  ap_demo.o(i.ap_set_hbm_53)
    ap_set_hbm_53                            0x00013111   Thumb Code    44  ap_demo.o(i.ap_set_hbm_53)
    i.ap_update_frame_rate                   0x00013140   Section        0  ap_demo.o(i.ap_update_frame_rate)
    ap_update_frame_rate                     0x00013141   Thumb Code    36  ap_demo.o(i.ap_update_frame_rate)
    i.app_ADC_IRQn_Handler                   0x00013168   Section        0  drv_rxbr.o(i.app_ADC_IRQn_Handler)
    i.app_AP_NRESET_IRQn_Handler             0x00013184   Section        0  drv_gpio.o(i.app_AP_NRESET_IRQn_Handler)
    i.app_EXTI_INT0_IRQn_Handler             0x000131a8   Section        0  drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler)
    i.app_EXTI_INT1_IRQn_Handler             0x000131c4   Section        0  drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler)
    i.app_EXTI_INT2_IRQn_Handler             0x000131e0   Section        0  drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler)
    i.app_EXTI_INT3_IRQn_Handler             0x000131fc   Section        0  drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler)
    i.app_EXTI_INT4_IRQn_Handler             0x00013218   Section        0  drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler)
    i.app_EXTI_INT5_IRQn_Handler             0x00013234   Section        0  drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler)
    i.app_EXTI_INT6_IRQn_Handler             0x00013250   Section        0  drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler)
    i.app_EXTI_INT7_IRQn_Handler             0x0001326c   Section        0  drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler)
    i.app_HardFault_Handler                  0x00013288   Section        0  drv_common.o(i.app_HardFault_Handler)
    i.app_I2C0_IRQn_Handler                  0x000132d0   Section        0  drv_i2c_slave.o(i.app_I2C0_IRQn_Handler)
    i.app_I2C1_IRQn_Handler                  0x000132e8   Section        0  drv_i2c_master.o(i.app_I2C1_IRQn_Handler)
    i.app_LCDC_IRQn_Handler                  0x000132f8   Section        0  hal_internal_vsync.o(i.app_LCDC_IRQn_Handler)
    i.app_MEMC_IRQn_Handler                  0x00013428   Section        0  drv_memc.o(i.app_MEMC_IRQn_Handler)
    i.app_MIPI_RX_IRQn_Handler               0x000134b0   Section        0  drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler)
    i.app_MIPI_TX_IRQn_Handler               0x00013748   Section        0  drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler)
    i.app_PWMDET_IRQn_Handler                0x000137e8   Section        0  drv_pwm.o(i.app_PWMDET_IRQn_Handler)
    i.app_SPIM_IRQn_Handler                  0x00013830   Section        0  drv_spi_master.o(i.app_SPIM_IRQn_Handler)
    i.app_SPIS_IRQn_Handler                  0x00013860   Section        0  hal_spi_slave.o(i.app_SPIS_IRQn_Handler)
    i.app_SWIRE_IRQn_Handler                 0x00013a60   Section        0  drv_swire.o(i.app_SWIRE_IRQn_Handler)
    i.app_SysTick_Handler                    0x00013a80   Section        0  drv_common.o(i.app_SysTick_Handler)
    i.app_TIMER0_IRQn_Handler                0x00013a98   Section        0  drv_timer.o(i.app_TIMER0_IRQn_Handler)
    i.app_TIMER1_IRQn_Handler                0x00013aa2   Section        0  drv_timer.o(i.app_TIMER1_IRQn_Handler)
    i.app_TIMER2_IRQn_Handler                0x00013aac   Section        0  drv_timer.o(i.app_TIMER2_IRQn_Handler)
    i.app_TIMER3_IRQn_Handler                0x00013ab6   Section        0  drv_timer.o(i.app_TIMER3_IRQn_Handler)
    i.app_UART_IRQn_Handler                  0x00013ac0   Section        0  drv_uart.o(i.app_UART_IRQn_Handler)
    i.app_VIDC_IRQn_Handler                  0x00013ac8   Section        0  drv_vidc.o(i.app_VIDC_IRQn_Handler)
    i.app_VPRE_IRQn_Handler                  0x00013ae4   Section        0  drv_rxbr.o(i.app_VPRE_IRQn_Handler)
    i.app_WDG_IRQn_Handler                   0x00013b00   Section        0  drv_wdg.o(i.app_WDG_IRQn_Handler)
    i.app_dma_irq_handler                    0x00013b38   Section        0  drv_dma.o(i.app_dma_irq_handler)
    i.app_fls_ctrl_Handler                   0x00013b48   Section        0  norflash.o(i.app_fls_ctrl_Handler)
    i.board_Init                             0x00013b78   Section        0  board.o(i.board_Init)
    i.calc_framebuffer_setting               0x00013b9c   Section        0  hal_internal_vsync.o(i.calc_framebuffer_setting)
    i.ceil                                   0x00014128   Section        0  ceil.o(i.ceil)
    i.check_mipi_rx_tx_video_info            0x000141f0   Section        0  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    check_mipi_rx_tx_video_info              0x000141f1   Thumb Code    44  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    i.check_pkt_buf_rev                      0x0001421c   Section        0  hal_internal_vsync.o(i.check_pkt_buf_rev)
    check_pkt_buf_rev                        0x0001421d   Thumb Code    74  hal_internal_vsync.o(i.check_pkt_buf_rev)
    i.dcs_packet_fifo_alloc                  0x000142a0   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    i.dcs_packet_fifo_init                   0x000142f8   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    i.dcs_packet_free_fifo_header            0x00014310   Section        0  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    i.dcs_packet_get_fifo_header             0x00014354   Section        0  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    i.dcs_sw_filter                          0x00014378   Section        0  hal_internal_vsync.o(i.dcs_sw_filter)
    dcs_sw_filter                            0x00014379   Thumb Code    36  hal_internal_vsync.o(i.dcs_sw_filter)
    i.delayMs                                0x000143a4   Section        0  tau_delay.o(i.delayMs)
    i.delayUs                                0x000143bc   Section        0  tau_delay.o(i.delayUs)
    i.drv_ap_rst_trig_edge_detect            0x000143e0   Section        0  drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect)
    i.drv_chip_info_get_info                 0x00014418   Section        0  drv_chip_info.o(i.drv_chip_info_get_info)
    i.drv_chip_info_init                     0x00014424   Section        0  drv_chip_info.o(i.drv_chip_info_init)
    i.drv_chip_rx_info_check                 0x00014464   Section        0  drv_chip_info.o(i.drv_chip_rx_info_check)
    i.drv_chip_rx_init_done                  0x00014514   Section        0  drv_chip_info.o(i.drv_chip_rx_init_done)
    i.drv_common_enable_systick              0x00014528   Section        0  drv_common.o(i.drv_common_enable_systick)
    i.drv_common_get_tick                    0x00014580   Section        0  drv_common.o(i.drv_common_get_tick)
    i.drv_common_system_init                 0x0001458c   Section        0  drv_common.o(i.drv_common_system_init)
    i.drv_crgu_config_reset_modules          0x00014594   Section        0  drv_crgu.o(i.drv_crgu_config_reset_modules)
    i.drv_crgu_set_ahb_pre_div               0x000145a4   Section        0  drv_crgu.o(i.drv_crgu_set_ahb_pre_div)
    i.drv_crgu_set_ahb_src                   0x000145b8   Section        0  drv_crgu.o(i.drv_crgu_set_ahb_src)
    i.drv_crgu_set_clock                     0x000145cc   Section        0  drv_crgu.o(i.drv_crgu_set_clock)
    i.drv_crgu_set_dpi_mux_src               0x000145ec   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_mux_src)
    i.drv_crgu_set_dpi_pre_div               0x00014600   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_pre_div)
    i.drv_crgu_set_dpi_pre_src               0x00014618   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_pre_src)
    i.drv_crgu_set_dsc_core_div              0x0001462c   Section        0  drv_crgu.o(i.drv_crgu_set_dsc_core_div)
    i.drv_crgu_set_dsco_src                  0x00014640   Section        0  drv_crgu.o(i.drv_crgu_set_dsco_src)
    i.drv_crgu_set_dsco_src_div              0x00014654   Section        0  drv_crgu.o(i.drv_crgu_set_dsco_src_div)
    i.drv_crgu_set_fb_div                    0x00014668   Section        0  drv_crgu.o(i.drv_crgu_set_fb_div)
    i.drv_crgu_set_fb_src                    0x0001467c   Section        0  drv_crgu.o(i.drv_crgu_set_fb_src)
    i.drv_crgu_set_lcdc_div                  0x00014690   Section        0  drv_crgu.o(i.drv_crgu_set_lcdc_div)
    i.drv_crgu_set_lcdc_src                  0x000146a4   Section        0  drv_crgu.o(i.drv_crgu_set_lcdc_src)
    i.drv_crgu_set_mipi_cfg_src              0x000146b8   Section        0  drv_crgu.o(i.drv_crgu_set_mipi_cfg_src)
    i.drv_crgu_set_mipi_ref_src              0x000146cc   Section        0  drv_crgu.o(i.drv_crgu_set_mipi_ref_src)
    i.drv_crgu_set_reset                     0x000146e4   Section        0  drv_crgu.o(i.drv_crgu_set_reset)
    i.drv_crgu_set_rxbr_div                  0x000146fc   Section        0  drv_crgu.o(i.drv_crgu_set_rxbr_div)
    i.drv_crgu_set_rxbr_src                  0x00014710   Section        0  drv_crgu.o(i.drv_crgu_set_rxbr_src)
    i.drv_crgu_set_vidc_src                  0x00014724   Section        0  drv_crgu.o(i.drv_crgu_set_vidc_src)
    i.drv_dma_clear_flag                     0x00014738   Section        0  drv_dma.o(i.drv_dma_clear_flag)
    i.drv_dma_get_channel_flag               0x00014750   Section        0  drv_dma.o(i.drv_dma_get_channel_flag)
    i.drv_dma_irq_handler                    0x0001475c   Section        0  drv_dma.o(i.drv_dma_irq_handler)
    i.drv_dsc_dec_convert_pps_rc_parameter   0x000147ec   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter)
    i.drv_dsc_dec_disable                    0x00014822   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    i.drv_dsc_dec_enable                     0x00014830   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    i.drv_dsc_dec_get_nslc                   0x000148a4   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    i.drv_dsc_dec_set_u8_pps                 0x000148ae   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps)
    i.drv_dsi_rx_calc_ipi_tx_delay           0x000148d8   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    i.drv_dsi_rx_enable_irq                  0x000149dc   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    i.drv_dsi_rx_get_bta_status              0x00014a1c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_bta_status)
    i.drv_dsi_rx_get_color_bpp               0x00014a2c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    drv_dsi_rx_get_color_bpp                 0x00014a2d   Thumb Code    62  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    i.drv_dsi_rx_get_color_pcc               0x00014a7c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    drv_dsi_rx_get_color_pcc                 0x00014a7d   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    i.drv_dsi_rx_get_compression_en          0x00014a98   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    i.drv_dsi_rx_get_max_ret_size            0x00014aa0   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size)
    i.drv_dsi_rx_power_up                    0x00014aa6   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    i.drv_dsi_rx_set_ctrl_cfg                0x00014ab4   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    i.drv_dsi_rx_set_ddi_cfg                 0x00014ad4   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    i.drv_dsi_rx_set_ipi_cfg                 0x00014ae4   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    i.drv_dsi_rx_set_lane_swap               0x00014af4   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    i.drv_dsi_rx_set_resp_cnt                0x00014b3a   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    i.drv_dsi_rx_set_up_phy                  0x00014b60   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    i.drv_dsi_rx_shut_down                   0x00014c64   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    i.drv_dsi_tx_command_header              0x00014c72   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    i.drv_dsi_tx_command_mode_cfg            0x00014c86   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    i.drv_dsi_tx_config_eotp                 0x00014cf2   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    i.drv_dsi_tx_config_int                  0x00014d0a   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    i.drv_dsi_tx_dpi_lpcmd_time              0x00014d12   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    i.drv_dsi_tx_dpi_mode                    0x00014d1a   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    i.drv_dsi_tx_dpi_polarity                0x00014d24   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    i.drv_dsi_tx_edpi_cmd_size               0x00014d48   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    i.drv_dsi_tx_get_cmd_status              0x00014d4c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    i.drv_dsi_tx_mode                        0x00014d50   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    i.drv_dsi_tx_phy_clock_lane_auto_lp      0x00014d54   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    i.drv_dsi_tx_phy_clock_lane_req_hs       0x00014d6c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    i.drv_dsi_tx_phy_lane_mode               0x00014d86   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    i.drv_dsi_tx_phy_status_ready            0x00014d92   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    i.drv_dsi_tx_phy_status_stopstate        0x00014df6   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    i.drv_dsi_tx_phy_test_setup              0x00014e34   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    i.drv_dsi_tx_phy_time_cfg                0x00014f68   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    i.drv_dsi_tx_powerup                     0x00014f86   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    i.drv_dsi_tx_response_mode               0x00014f8e   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    i.drv_dsi_tx_set_bta_ack                 0x00014faa   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    i.drv_dsi_tx_set_esc_div                 0x00014fc2   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    i.drv_dsi_tx_set_int                     0x00014fd0   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    i.drv_dsi_tx_set_time_out_div            0x00015010   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    i.drv_dsi_tx_set_video_chunk             0x00015020   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    i.drv_dsi_tx_set_video_timing            0x00015028   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    i.drv_dsi_tx_shutdown                    0x0001504a   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    i.drv_dsi_tx_timeout_cfg                 0x00015052   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    i.drv_dsi_tx_video_mode_cfg              0x00015078   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    i.drv_dsi_tx_video_mode_disable_hact_cmd 0x00015122   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_disable_hact_cmd)
    i.drv_dsi_tx_video_mode_set_lp_cmd       0x00015138   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd)
    i.drv_efuse_enter_inactive               0x00015150   Section        0  drv_efuse.o(i.drv_efuse_enter_inactive)
    i.drv_efuse_int_enable                   0x0001517e   Section        0  drv_efuse.o(i.drv_efuse_int_enable)
    i.drv_efuse_read                         0x0001518a   Section        0  drv_efuse.o(i.drv_efuse_read)
    i.drv_efuse_read_req                     0x000151bc   Section        0  drv_efuse.o(i.drv_efuse_read_req)
    i.drv_gpio_get_input_data                0x000151d4   Section        0  drv_gpio.o(i.drv_gpio_get_input_data)
    i.drv_gpio_set_ioe                       0x000151ec   Section        0  drv_gpio.o(i.drv_gpio_set_ioe)
    i.drv_gpio_set_mode0                     0x0001520c   Section        0  drv_gpio.o(i.drv_gpio_set_mode0)
    i.drv_gpio_set_mode1                     0x0001521c   Section        0  drv_gpio.o(i.drv_gpio_set_mode1)
    i.drv_gpio_set_mode2                     0x0001522c   Section        0  drv_gpio.o(i.drv_gpio_set_mode2)
    i.drv_gpio_set_mode3                     0x0001523c   Section        0  drv_gpio.o(i.drv_gpio_set_mode3)
    i.drv_gpio_set_output_data               0x0001524c   Section        0  hal_gpio.o(i.drv_gpio_set_output_data)
    drv_gpio_set_output_data                 0x0001524d   Thumb Code    26  hal_gpio.o(i.drv_gpio_set_output_data)
    i.drv_gpio_set_pull_state                0x0001526c   Section        0  drv_gpio.o(i.drv_gpio_set_pull_state)
    i.drv_lcdc_config_bypass                 0x0001539c   Section        0  drv_lcdc.o(i.drv_lcdc_config_bypass)
    i.drv_lcdc_config_ccm                    0x000153b4   Section        0  drv_lcdc.o(i.drv_lcdc_config_ccm)
    i.drv_lcdc_config_disp_mode              0x000153e4   Section        0  drv_lcdc.o(i.drv_lcdc_config_disp_mode)
    i.drv_lcdc_config_dpi_polarity           0x000153fa   Section        0  drv_lcdc.o(i.drv_lcdc_config_dpi_polarity)
    i.drv_lcdc_config_dpi_timing             0x0001541e   Section        0  drv_lcdc.o(i.drv_lcdc_config_dpi_timing)
    i.drv_lcdc_config_edpi_mode              0x00015444   Section        0  drv_lcdc.o(i.drv_lcdc_config_edpi_mode)
    i.drv_lcdc_config_endianness             0x0001545a   Section        0  drv_lcdc.o(i.drv_lcdc_config_endianness)
    i.drv_lcdc_config_input_size             0x00015470   Section        0  drv_lcdc.o(i.drv_lcdc_config_input_size)
    i.drv_lcdc_config_int                    0x0001547c   Section        0  drv_lcdc.o(i.drv_lcdc_config_int)
    i.drv_lcdc_config_int_single             0x0001549a   Section        0  drv_lcdc.o(i.drv_lcdc_config_int_single)
    i.drv_lcdc_config_overwrite              0x000154bc   Section        0  drv_lcdc.o(i.drv_lcdc_config_overwrite)
    i.drv_lcdc_config_overwrite_rgb          0x000154de   Section        0  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    i.drv_lcdc_config_partial_display_area   0x000154ea   Section        0  drv_lcdc.o(i.drv_lcdc_config_partial_display_area)
    i.drv_lcdc_config_partial_display_enable 0x00015504   Section        0  drv_lcdc.o(i.drv_lcdc_config_partial_display_enable)
    i.drv_lcdc_config_scale_up_coef          0x00015526   Section        0  drv_lcdc.o(i.drv_lcdc_config_scale_up_coef)
    i.drv_lcdc_config_scale_up_step          0x00015540   Section        0  drv_lcdc.o(i.drv_lcdc_config_scale_up_step)
    i.drv_lcdc_config_src_parameter          0x0001554c   Section        0  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    i.drv_lcdc_config_thresh                 0x00015598   Section        0  drv_lcdc.o(i.drv_lcdc_config_thresh)
    i.drv_lcdc_ctrl_flow                     0x0001559e   Section        0  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    i.drv_lcdc_enable_shadow_reg             0x000155b0   Section        0  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    i.drv_lcdc_set_int                       0x000155d0   Section        0  drv_lcdc.o(i.drv_lcdc_set_int)
    i.drv_lcdc_set_prefetch                  0x00015610   Section        0  drv_lcdc.o(i.drv_lcdc_set_prefetch)
    i.drv_lcdc_set_video_hw_mode             0x00015628   Section        0  drv_lcdc.o(i.drv_lcdc_set_video_hw_mode)
    i.drv_lcdc_start                         0x0001563c   Section        0  drv_lcdc.o(i.drv_lcdc_start)
    i.drv_memc_clear_status                  0x0001565c   Section        0  drv_memc.o(i.drv_memc_clear_status)
    i.drv_memc_enable_irq                    0x00015668   Section        0  drv_memc.o(i.drv_memc_enable_irq)
    i.drv_memc_gen_a_tear_signal             0x000156a8   Section        0  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    i.drv_memc_get_status                    0x000156b4   Section        0  drv_memc.o(i.drv_memc_get_status)
    i.drv_memc_rate_transfer_sel             0x000156c6   Section        0  drv_memc.o(i.drv_memc_rate_transfer_sel)
    i.drv_memc_sel_vsync                     0x000156d6   Section        0  drv_memc.o(i.drv_memc_sel_vsync)
    i.drv_memc_set_active_height             0x000156e4   Section        0  drv_memc.o(i.drv_memc_set_active_height)
    i.drv_memc_set_data_mode                 0x000156f8   Section        0  drv_memc.o(i.drv_memc_set_data_mode)
    i.drv_memc_set_double_buffer             0x00015704   Section        0  drv_memc.o(i.drv_memc_set_double_buffer)
    i.drv_memc_set_double_buffer_reverse     0x00015714   Section        0  drv_memc.o(i.drv_memc_set_double_buffer_reverse)
    i.drv_memc_set_fs_en_conditions          0x00015726   Section        0  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    i.drv_memc_set_inten                     0x00015736   Section        0  drv_memc.o(i.drv_memc_set_inten)
    i.drv_memc_set_lcdc_st_conditions        0x0001574c   Section        0  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    i.drv_memc_set_ltpo_mode                 0x00015764   Section        0  drv_memc.o(i.drv_memc_set_ltpo_mode)
    i.drv_memc_set_tear_mode                 0x0001577e   Section        0  drv_memc.o(i.drv_memc_set_tear_mode)
    i.drv_memc_set_tear_waveform             0x0001578c   Section        0  drv_memc.o(i.drv_memc_set_tear_waveform)
    i.drv_memc_set_vidc_sync_cnt             0x000157b4   Section        0  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    i.drv_param_init_get_ccm                 0x000157c4   Section        0  drv_param_init.o(i.drv_param_init_get_ccm)
    i.drv_param_init_get_scld_filter_h       0x000157cc   Section        0  drv_param_init.o(i.drv_param_init_get_scld_filter_h)
    i.drv_param_init_get_scld_filter_v       0x000157e0   Section        0  drv_param_init.o(i.drv_param_init_get_scld_filter_v)
    i.drv_param_init_get_sclu_filter         0x000157f4   Section        0  drv_param_init.o(i.drv_param_init_get_sclu_filter)
    i.drv_param_init_set_ccm                 0x000157fc   Section        0  drv_param_init.o(i.drv_param_init_set_ccm)
    i.drv_param_init_set_scld_filter         0x00015810   Section        0  drv_param_init.o(i.drv_param_init_set_scld_filter)
    i.drv_param_p2r_filter_init              0x00015874   Section        0  drv_param_init.o(i.drv_param_p2r_filter_init)
    i.drv_phy_enable_calibration             0x00015898   Section        0  drv_phy_common.o(i.drv_phy_enable_calibration)
    i.drv_phy_get_calibration                0x000158a8   Section        0  drv_phy_common.o(i.drv_phy_get_calibration)
    i.drv_phy_get_pll_para                   0x000158e4   Section        0  drv_phy_common.o(i.drv_phy_get_pll_para)
    i.drv_phy_get_rate_para                  0x00015944   Section        0  drv_phy_common.o(i.drv_phy_get_rate_para)
    i.drv_phy_test_clear                     0x00015998   Section        0  drv_phy_common.o(i.drv_phy_test_clear)
    i.drv_phy_test_lock                      0x000159a8   Section        0  drv_phy_common.o(i.drv_phy_test_lock)
    i.drv_phy_test_write_1_byte              0x000159c0   Section        0  drv_phy_common.o(i.drv_phy_test_write_1_byte)
    i.drv_phy_test_write_2_byte              0x000159e0   Section        0  drv_phy_common.o(i.drv_phy_test_write_2_byte)
    i.drv_phy_test_write_code                0x00015a06   Section        0  drv_phy_common.o(i.drv_phy_test_write_code)
    i.drv_phy_test_write_data                0x00015a24   Section        0  drv_phy_common.o(i.drv_phy_test_write_data)
    drv_phy_test_write_data                  0x00015a25   Thumb Code    32  drv_phy_common.o(i.drv_phy_test_write_data)
    i.drv_pwr_set_pvd_mode                   0x00015a44   Section        0  drv_pwr.o(i.drv_pwr_set_pvd_mode)
    i.drv_pwr_set_system_clk_src             0x00015a5c   Section        0  drv_pwr.o(i.drv_pwr_set_system_clk_src)
    i.drv_rx_phy_test_clear                  0x00015a94   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_clear)
    drv_rx_phy_test_clear                    0x00015a95   Thumb Code    12  drv_dsi_rx.o(i.drv_rx_phy_test_clear)
    i.drv_rx_phy_test_lock                   0x00015aa0   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_lock)
    drv_rx_phy_test_lock                     0x00015aa1   Thumb Code    16  drv_dsi_rx.o(i.drv_rx_phy_test_lock)
    i.drv_rx_phy_test_write_1_byte           0x00015ab0   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte)
    drv_rx_phy_test_write_1_byte             0x00015ab1   Thumb Code    20  drv_dsi_rx.o(i.drv_rx_phy_test_write_1_byte)
    i.drv_rx_phy_test_write_2_byte           0x00015ac4   Section        0  drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte)
    drv_rx_phy_test_write_2_byte             0x00015ac5   Thumb Code    22  drv_dsi_rx.o(i.drv_rx_phy_test_write_2_byte)
    i.drv_rxbr_clear_pkt_buffer              0x00015ada   Section        0  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    i.drv_rxbr_clear_status0                 0x00015ae4   Section        0  drv_rxbr.o(i.drv_rxbr_clear_status0)
    i.drv_rxbr_enable_irq                    0x00015ae8   Section        0  drv_rxbr.o(i.drv_rxbr_enable_irq)
    i.drv_rxbr_frame_drop_cfg                0x00015b44   Section        0  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    i.drv_rxbr_get_clk                       0x00015b58   Section        0  drv_rxbr.o(i.drv_rxbr_get_clk)
    i.drv_rxbr_get_col_addr                  0x00015bbc   Section        0  drv_rxbr.o(i.drv_rxbr_get_col_addr)
    i.drv_rxbr_get_int_source                0x00015bc0   Section        0  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    drv_rxbr_get_int_source                  0x00015bc1   Thumb Code    18  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    i.drv_rxbr_get_page_addr                 0x00015bd2   Section        0  drv_rxbr.o(i.drv_rxbr_get_page_addr)
    i.drv_rxbr_get_pkt_buf_error_status      0x00015bd6   Section        0  drv_rxbr.o(i.drv_rxbr_get_pkt_buf_error_status)
    i.drv_rxbr_get_status0                   0x00015be2   Section        0  hal_internal_vsync.o(i.drv_rxbr_get_status0)
    drv_rxbr_get_status0                     0x00015be3   Thumb Code    18  hal_internal_vsync.o(i.drv_rxbr_get_status0)
    i.drv_rxbr_get_status1                   0x00015bf4   Section        0  hal_internal_vsync.o(i.drv_rxbr_get_status1)
    drv_rxbr_get_status1                     0x00015bf5   Thumb Code    22  hal_internal_vsync.o(i.drv_rxbr_get_status1)
    i.drv_rxbr_hline_rcv0_cfg                0x00015c0a   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg)
    i.drv_rxbr_hline_rcv1_cfg                0x00015c16   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg)
    i.drv_rxbr_hline_rcv_cfg                 0x00015c22   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    i.drv_rxbr_register_irq0_callback        0x00015c2c   Section        0  drv_rxbr.o(i.drv_rxbr_register_irq0_callback)
    i.drv_rxbr_register_irq1_callback        0x00015c38   Section        0  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    i.drv_rxbr_set_ack_pkt_header            0x00015c44   Section        0  drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header)
    i.drv_rxbr_set_color_format              0x00015c58   Section        0  drv_rxbr.o(i.drv_rxbr_set_color_format)
    i.drv_rxbr_set_filter_regs               0x00015c6c   Section        0  drv_rxbr.o(i.drv_rxbr_set_filter_regs)
    i.drv_rxbr_set_inten                     0x00015c7e   Section        0  drv_rxbr.o(i.drv_rxbr_set_inten)
    i.drv_rxbr_set_ltpo_drop_th              0x00015c92   Section        0  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    i.drv_rxbr_set_usr_cfg                   0x00015ca2   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    i.drv_rxbr_set_usr_col                   0x00015cc8   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    i.drv_rxbr_set_usr_row                   0x00015cd0   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    i.drv_swire_set_int                      0x00015cd8   Section        0  drv_swire.o(i.drv_swire_set_int)
    i.drv_sys_cfg_clear_all_int              0x00015d2c   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    i.drv_sys_cfg_clear_pending              0x00015d38   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    i.drv_sys_cfg_sel_ap_rst_lvl_trig        0x00015d60   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig)
    i.drv_sys_cfg_set_int                    0x00015d78   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    i.drv_timer_clear_status_flags           0x00015d9c   Section        0  drv_timer.o(i.drv_timer_clear_status_flags)
    drv_timer_clear_status_flags             0x00015d9d   Thumb Code    26  drv_timer.o(i.drv_timer_clear_status_flags)
    i.drv_timer_enable                       0x00015db6   Section        0  drv_timer.o(i.drv_timer_enable)
    i.drv_timer_get_instance                 0x00015dd8   Section        0  drv_timer.o(i.drv_timer_get_instance)
    i.drv_timer_handle_interrupt             0x00015de8   Section        0  drv_timer.o(i.drv_timer_handle_interrupt)
    drv_timer_handle_interrupt               0x00015de9   Thumb Code    62  drv_timer.o(i.drv_timer_handle_interrupt)
    i.drv_timer_set_compare_val              0x00015e2c   Section        0  drv_timer.o(i.drv_timer_set_compare_val)
    i.drv_timer_set_int                      0x00015e3c   Section        0  drv_timer.o(i.drv_timer_set_int)
    i.drv_tx_phy_test_clear                  0x00015e90   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_clear)
    drv_tx_phy_test_clear                    0x00015e91   Thumb Code    10  drv_dsi_tx.o(i.drv_tx_phy_test_clear)
    i.drv_tx_phy_test_enter                  0x00015e9a   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    i.drv_tx_phy_test_exit                   0x00015eb6   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    i.drv_tx_phy_test_write_1_byte           0x00015ed2   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte)
    drv_tx_phy_test_write_1_byte             0x00015ed3   Thumb Code    18  drv_dsi_tx.o(i.drv_tx_phy_test_write_1_byte)
    i.drv_tx_phy_test_write_2_byte           0x00015ee4   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte)
    drv_tx_phy_test_write_2_byte             0x00015ee5   Thumb Code    20  drv_dsi_tx.o(i.drv_tx_phy_test_write_2_byte)
    i.drv_tx_phy_test_write_code             0x00015ef8   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    drv_tx_phy_test_write_code               0x00015ef9   Thumb Code    16  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    i.drv_vidc_clear_irq                     0x00015f08   Section        0  drv_vidc.o(i.drv_vidc_clear_irq)
    i.drv_vidc_enable                        0x00015f10   Section        0  drv_vidc.o(i.drv_vidc_enable)
    i.drv_vidc_enable_irq                    0x00015f28   Section        0  drv_vidc.o(i.drv_vidc_enable_irq)
    i.drv_vidc_get_irq_status                0x00015f68   Section        0  drv_vidc.o(i.drv_vidc_get_irq_status)
    i.drv_vidc_init_module_enable            0x00015f7c   Section        0  drv_vidc.o(i.drv_vidc_init_module_enable)
    i.drv_vidc_register_callback             0x00015fa4   Section        0  drv_vidc.o(i.drv_vidc_register_callback)
    i.drv_vidc_reset                         0x00015fb0   Section        0  drv_vidc.o(i.drv_vidc_reset)
    i.drv_vidc_set_dst_parameter             0x00015fb6   Section        0  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    i.drv_vidc_set_irqen                     0x00015ff2   Section        0  drv_vidc.o(i.drv_vidc_set_irqen)
    i.drv_vidc_set_mirror                    0x00016006   Section        0  drv_vidc.o(i.drv_vidc_set_mirror)
    i.drv_vidc_set_p2r_hcoef0                0x00016016   Section        0  drv_vidc.o(i.drv_vidc_set_p2r_hcoef0)
    i.drv_vidc_set_p2r_hinitb                0x0001601e   Section        0  drv_vidc.o(i.drv_vidc_set_p2r_hinitb)
    i.drv_vidc_set_p2r_hinitr                0x00016044   Section        0  drv_vidc.o(i.drv_vidc_set_p2r_hinitr)
    i.drv_vidc_set_pentile_swap              0x0001606c   Section        0  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    i.drv_vidc_set_pu_ctrl                   0x00016084   Section        0  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    i.drv_vidc_set_rotation                  0x0001608e   Section        0  drv_vidc.o(i.drv_vidc_set_rotation)
    i.drv_vidc_set_scld_hcoef0               0x0001609e   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    i.drv_vidc_set_scld_hcoef1               0x000160a8   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    i.drv_vidc_set_scld_step                 0x000160b2   Section        0  drv_vidc.o(i.drv_vidc_set_scld_step)
    i.drv_vidc_set_scld_vcoef0               0x000160c4   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    i.drv_vidc_set_scld_vcoef1               0x000160ce   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    i.drv_vidc_set_src_parameter             0x000160d8   Section        0  drv_vidc.o(i.drv_vidc_set_src_parameter)
    i.drv_wdg_clear_counter                  0x000160f0   Section        0  drv_wdg.o(i.drv_wdg_clear_counter)
    i.drv_wdg_clear_edge_flag                0x00016100   Section        0  drv_wdg.o(i.drv_wdg_clear_edge_flag)
    drv_wdg_clear_edge_flag                  0x00016101   Thumb Code    12  drv_wdg.o(i.drv_wdg_clear_edge_flag)
    i.drv_wdg_read_edge_flag                 0x00016110   Section        0  drv_wdg.o(i.drv_wdg_read_edge_flag)
    drv_wdg_read_edge_flag                   0x00016111   Thumb Code    10  drv_wdg.o(i.drv_wdg_read_edge_flag)
    i.drv_wdg_set_int                        0x00016120   Section        0  drv_wdg.o(i.drv_wdg_set_int)
    i.fls_clr_interrupt_flag                 0x00016160   Section        0  drv_fls.o(i.fls_clr_interrupt_flag)
    i.fputc                                  0x0001616a   Section        0  tau_log.o(i.fputc)
    i.frame_start_cb                         0x00016180   Section        0  ap_demo.o(i.frame_start_cb)
    frame_start_cb                           0x00016181   Thumb Code    38  ap_demo.o(i.frame_start_cb)
    i.hal_dsi_rx_ctrl_create_handle          0x000161d0   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    i.hal_dsi_rx_ctrl_dsc_async_handler      0x00016204   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler)
    i.hal_dsi_rx_ctrl_gen_a_tear_signal      0x0001622c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal)
    i.hal_dsi_rx_ctrl_get_max_ret_size       0x00016254   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size)
    i.hal_dsi_rx_ctrl_init                   0x0001627c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    i.hal_dsi_rx_ctrl_init_clk               0x00016314   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    hal_dsi_rx_ctrl_init_clk                 0x00016315   Thumb Code   332  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    i.hal_dsi_rx_ctrl_init_dsi_rx            0x000164b8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    hal_dsi_rx_ctrl_init_dsi_rx              0x000164b9   Thumb Code   184  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    i.hal_dsi_rx_ctrl_init_memc              0x00016590   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    hal_dsi_rx_ctrl_init_memc                0x00016591   Thumb Code   342  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    i.hal_dsi_rx_ctrl_init_rxbr              0x000166f0   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    hal_dsi_rx_ctrl_init_rxbr                0x000166f1   Thumb Code   320  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    i.hal_dsi_rx_ctrl_init_vidc              0x00016840   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    hal_dsi_rx_ctrl_init_vidc                0x00016841   Thumb Code   544  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    i.hal_dsi_rx_ctrl_pre_init_pps           0x00016a6c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    i.hal_dsi_rx_ctrl_restart                0x00016aa8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart)
    i.hal_dsi_rx_ctrl_send_ack_cmd           0x00016af8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd)
    i.hal_dsi_rx_ctrl_set_cus_esc_clk        0x00016be8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk)
    i.hal_dsi_rx_ctrl_set_cus_scld_filter    0x00016c14   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter)
    i.hal_dsi_rx_ctrl_set_cus_sync_line      0x00016c80   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line)
    i.hal_dsi_rx_ctrl_set_ipi_cfg            0x00016cb4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    hal_dsi_rx_ctrl_set_ipi_cfg              0x00016cb5   Thumb Code    50  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    i.hal_dsi_rx_ctrl_set_rxbr_clk           0x00016cec   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk)
    hal_dsi_rx_ctrl_set_rxbr_clk             0x00016ced   Thumb Code   114  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk)
    i.hal_dsi_rx_ctrl_set_tear_mode_ex       0x00016d5e   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex)
    i.hal_dsi_rx_ctrl_start                  0x00016d6c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    i.hal_dsi_rx_ctrl_toggle_resolution      0x00016da8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    i.hal_dsi_tx_calc_video_chunks           0x00016dc8   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks)
    hal_dsi_tx_calc_video_chunks             0x00016dc9   Thumb Code   384  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_calc_video_chunks)
    i.hal_dsi_tx_config_params_for_lane_rate 0x00016f58   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate)
    hal_dsi_tx_config_params_for_lane_rate   0x00016f59   Thumb Code    42  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_config_params_for_lane_rate)
    i.hal_dsi_tx_count_lane_rate             0x00016f8c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate)
    hal_dsi_tx_count_lane_rate               0x00016f8d   Thumb Code   982  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_count_lane_rate)
    i.hal_dsi_tx_ctrl_create_handle          0x000173b4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    i.hal_dsi_tx_ctrl_enter_init_panel_mode  0x000173e0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode)
    i.hal_dsi_tx_ctrl_exit_init_panel_mode   0x0001742c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode)
    i.hal_dsi_tx_ctrl_init                   0x00017454   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    i.hal_dsi_tx_ctrl_init_clk               0x000174f8   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    hal_dsi_tx_ctrl_init_clk                 0x000174f9   Thumb Code    36  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    i.hal_dsi_tx_ctrl_panel_reset_pin        0x0001751c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin)
    i.hal_dsi_tx_ctrl_set_ccm                0x00017528   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm)
    i.hal_dsi_tx_ctrl_set_overwrite_rgb      0x00017548   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    i.hal_dsi_tx_ctrl_set_partial_disp       0x0001755c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp)
    i.hal_dsi_tx_ctrl_set_partial_disp_area  0x0001756c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area)
    i.hal_dsi_tx_ctrl_start                  0x00017590   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    i.hal_dsi_tx_ctrl_write_array_cmd        0x00017638   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd)
    i.hal_dsi_tx_ctrl_write_cmd              0x00017728   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    i.hal_dsi_tx_init_data_mode              0x000177f4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode)
    hal_dsi_tx_init_data_mode                0x000177f5   Thumb Code    58  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_data_mode)
    i.hal_dsi_tx_init_dpi_cfg                0x00017838   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg)
    hal_dsi_tx_init_dpi_cfg                  0x00017839   Thumb Code    42  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_cfg)
    i.hal_dsi_tx_init_interrupt              0x00017868   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt)
    hal_dsi_tx_init_interrupt                0x00017869   Thumb Code    28  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_interrupt)
    i.hal_dsi_tx_init_phy_cfg                0x00017888   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    hal_dsi_tx_init_phy_cfg                  0x00017889   Thumb Code    28  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    i.hal_dsi_tx_init_remains                0x000178a8   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains)
    hal_dsi_tx_init_remains                  0x000178a9   Thumb Code   142  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_remains)
    i.hal_dsi_tx_init_video_mode             0x0001793c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode)
    hal_dsi_tx_init_video_mode               0x0001793d   Thumb Code    82  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_video_mode)
    i.hal_dsi_tx_send_cmd                    0x00017994   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    hal_dsi_tx_send_cmd                      0x00017995   Thumb Code    60  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    i.hal_gpio_get_input_data                0x000179d8   Section        0  hal_gpio.o(i.hal_gpio_get_input_data)
    i.hal_gpio_init_input                    0x000179ec   Section        0  hal_gpio.o(i.hal_gpio_init_input)
    i.hal_gpio_init_output                   0x00017a0c   Section        0  hal_gpio.o(i.hal_gpio_init_output)
    i.hal_gpio_set_mode                      0x00017a34   Section        0  hal_gpio.o(i.hal_gpio_set_mode)
    i.hal_gpio_set_output_data               0x00017a94   Section        0  hal_gpio.o(i.hal_gpio_set_output_data)
    i.hal_gpio_set_pull_state                0x00017a9c   Section        0  hal_gpio.o(i.hal_gpio_set_pull_state)
    i.hal_internal_check_video_auto_sync     0x00017abc   Section        0  hal_internal_vsync.o(i.hal_internal_check_video_auto_sync)
    i.hal_internal_init_memc                 0x00017ad4   Section        0  hal_internal_vsync.o(i.hal_internal_init_memc)
    i.hal_internal_rx_dcs_async_handler      0x00017bd0   Section        0  hal_internal_vsync.o(i.hal_internal_rx_dcs_async_handler)
    i.hal_internal_rx_dcs_polling            0x00017bfc   Section        0  hal_internal_vsync.o(i.hal_internal_rx_dcs_polling)
    i.hal_internal_sync_get_fb_setting       0x00017c54   Section        0  hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting)
    i.hal_internal_sync_get_hight_performan_mode 0x00017c64   Section        0  hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode)
    i.hal_internal_sync_input_resolution_change 0x00017c74   Section        0  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    i.hal_internal_vsync_deinit              0x00017ea0   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    i.hal_internal_vsync_get_sync_line       0x00017ec8   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    i.hal_internal_vsync_get_tear_mode       0x00017ee0   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_tear_mode)
    i.hal_internal_vsync_get_tx_state        0x00017eec   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    i.hal_internal_vsync_init_rx             0x00017ef8   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    i.hal_internal_vsync_init_tx             0x00018038   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    i.hal_internal_vsync_set_auto_hw_filter  0x000180e8   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter)
    i.hal_internal_vsync_set_rx_state        0x00018178   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    i.hal_internal_vsync_set_sync_line       0x0001819c   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line)
    i.hal_internal_vsync_set_tear_mode       0x000181e0   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    i.hal_internal_vsync_set_tx_state        0x00018230   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    i.hal_intl_svs_deinit_tx                 0x000182b4   Section        0  hal_internal_soft_sync.o(i.hal_intl_svs_deinit_tx)
    i.hal_intl_svs_handle                    0x000182c4   Section        0  hal_internal_soft_sync.o(i.hal_intl_svs_handle)
    i.hal_intl_svs_init_rx                   0x000182e8   Section        0  hal_internal_soft_sync.o(i.hal_intl_svs_init_rx)
    i.hal_intl_svs_init_tx                   0x00018360   Section        0  hal_internal_soft_sync.o(i.hal_intl_svs_init_tx)
    i.hal_intl_svs_set_sync_coef             0x00018374   Section        0  hal_internal_soft_sync.o(i.hal_intl_svs_set_sync_coef)
    i.hal_intl_svs_update_rxbr_clk           0x00018380   Section        0  hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk)
    i.hal_lcdc_config_ccm                    0x000183c8   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm)
    hal_lcdc_config_ccm                      0x000183c9   Thumb Code    30  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_ccm)
    i.hal_lcdc_config_remains                0x000183ec   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains)
    hal_lcdc_config_remains                  0x000183ed   Thumb Code    94  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_remains)
    i.hal_lcdc_config_rgb_to_pentile         0x00018450   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile)
    hal_lcdc_config_rgb_to_pentile           0x00018451   Thumb Code    14  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_rgb_to_pentile)
    i.hal_lcdc_config_upscaler               0x00018464   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler)
    hal_lcdc_config_upscaler                 0x00018465   Thumb Code   348  hal_dsi_tx_ctrl.o(i.hal_lcdc_config_upscaler)
    i.hal_lcdc_init_cfg                      0x000185c8   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    hal_lcdc_init_cfg                        0x000185c9   Thumb Code    78  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    i.hal_lcdc_init_clk                      0x0001861c   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    hal_lcdc_init_clk                        0x0001861d   Thumb Code   446  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    i.hal_lcdc_init_interrupt                0x000187e8   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt)
    hal_lcdc_init_interrupt                  0x000187e9   Thumb Code    58  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_interrupt)
    i.hal_system_enable_systick              0x00018828   Section        0  hal_system.o(i.hal_system_enable_systick)
    i.hal_system_get_tick                    0x00018830   Section        0  hal_system.o(i.hal_system_get_tick)
    i.hal_system_init                        0x00018838   Section        0  hal_system.o(i.hal_system_init)
    i.hal_system_init_console                0x000188c0   Section        0  hal_system.o(i.hal_system_init_console)
    i.hal_system_set_phy_calibration         0x000188dc   Section        0  hal_system.o(i.hal_system_set_phy_calibration)
    i.hal_tx_frame_rate_adjust               0x000188e4   Section        0  hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust)
    hal_tx_frame_rate_adjust                 0x000188e5   Thumb Code    44  hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust)
    i.hal_uart_init                          0x00018914   Section        0  hal_uart.o(i.hal_uart_init)
    i.hal_uart_transmit_blocking             0x000189a0   Section        0  hal_uart.o(i.hal_uart_transmit_blocking)
    i.handle_init                            0x000189b0   Section        0  irq_redirect .o(i.handle_init)
    i.init_mipi_tx                           0x00018ac0   Section        0  ap_demo.o(i.init_mipi_tx)
    init_mipi_tx                             0x00018ac1   Thumb Code   100  ap_demo.o(i.init_mipi_tx)
    i.init_panel                             0x00018b2c   Section        0  ap_demo.o(i.init_panel)
    init_panel                               0x00018b2d   Thumb Code   150  ap_demo.o(i.init_panel)
    i.main                                   0x00018bcc   Section        0  main.o(i.main)
    i.open_mipi_rx                           0x00018bd8   Section        0  ap_demo.o(i.open_mipi_rx)
    open_mipi_rx                             0x00018bd9   Thumb Code   170  ap_demo.o(i.open_mipi_rx)
    i.pps_update_handle                      0x00018cac   Section        0  ap_demo.o(i.pps_update_handle)
    pps_update_handle                        0x00018cad   Thumb Code    78  ap_demo.o(i.pps_update_handle)
    i.rx_get_dcs_packet_data                 0x00018d48   Section        0  hal_internal_vsync.o(i.rx_get_dcs_packet_data)
    rx_get_dcs_packet_data                   0x00018d49   Thumb Code   654  hal_internal_vsync.o(i.rx_get_dcs_packet_data)
    i.rx_partial_update                      0x0001913c   Section        0  hal_internal_vsync.o(i.rx_partial_update)
    rx_partial_update                        0x0001913d   Thumb Code   348  hal_internal_vsync.o(i.rx_partial_update)
    i.rx_receive_packet                      0x000192a8   Section        0  hal_internal_vsync.o(i.rx_receive_packet)
    rx_receive_packet                        0x000192a9   Thumb Code   126  hal_internal_vsync.o(i.rx_receive_packet)
    i.rx_receive_pps                         0x00019334   Section        0  hal_internal_vsync.o(i.rx_receive_pps)
    rx_receive_pps                           0x00019335   Thumb Code   268  hal_internal_vsync.o(i.rx_receive_pps)
    i.rxbr_irq0_callback                     0x000194b4   Section        0  hal_internal_vsync.o(i.rxbr_irq0_callback)
    rxbr_irq0_callback                       0x000194b5   Thumb Code   192  hal_internal_vsync.o(i.rxbr_irq0_callback)
    i.rxbr_irq1_callback                     0x00019580   Section        0  hal_internal_vsync.o(i.rxbr_irq1_callback)
    rxbr_irq1_callback                       0x00019581   Thumb Code   392  hal_internal_vsync.o(i.rxbr_irq1_callback)
    i.soft_gen_te                            0x000197c4   Section        0  hal_internal_vsync.o(i.soft_gen_te)
    soft_gen_te                              0x000197c5   Thumb Code   166  hal_internal_vsync.o(i.soft_gen_te)
    i.soft_gen_te_double_buffer              0x00019888   Section        0  hal_internal_vsync.o(i.soft_gen_te_double_buffer)
    soft_gen_te_double_buffer                0x00019889   Thumb Code   166  hal_internal_vsync.o(i.soft_gen_te_double_buffer)
    i.sqrt                                   0x00019948   Section        0  sqrt.o(i.sqrt)
    i.svs_direct_mode_setting                0x00019990   Section        0  hal_internal_soft_sync.o(i.svs_direct_mode_setting)
    svs_direct_mode_setting                  0x00019991   Thumb Code   156  hal_internal_soft_sync.o(i.svs_direct_mode_setting)
    i.svs_get_rel_intv                       0x00019a3c   Section        0  hal_internal_soft_sync.o(i.svs_get_rel_intv)
    svs_get_rel_intv                         0x00019a3d   Thumb Code    20  hal_internal_soft_sync.o(i.svs_get_rel_intv)
    i.svs_sync_handle                        0x00019a58   Section        0  hal_internal_soft_sync.o(i.svs_sync_handle)
    svs_sync_handle                          0x00019a59   Thumb Code   158  hal_internal_soft_sync.o(i.svs_sync_handle)
    i.svs_wait_start                         0x00019b08   Section        0  hal_internal_soft_sync.o(i.svs_wait_start)
    svs_wait_start                           0x00019b09   Thumb Code   224  hal_internal_soft_sync.o(i.svs_wait_start)
    i.svs_waite_fr_stab                      0x00019bfc   Section        0  hal_internal_soft_sync.o(i.svs_waite_fr_stab)
    svs_waite_fr_stab                        0x00019bfd   Thumb Code   148  hal_internal_soft_sync.o(i.svs_waite_fr_stab)
    i.vidc_callback                          0x00019cd4   Section        0  hal_internal_vsync.o(i.vidc_callback)
    vidc_callback                            0x00019cd5   Thumb Code   234  hal_internal_vsync.o(i.vidc_callback)
    i.vpre_err_reset                         0x00019ddc   Section        0  hal_internal_vsync.o(i.vpre_err_reset)
    vpre_err_reset                           0x00019ddd   Thumb Code   192  hal_internal_vsync.o(i.vpre_err_reset)
    i.vsync_set_te_mode                      0x00019eb4   Section        0  hal_internal_vsync.o(i.vsync_set_te_mode)
    vsync_set_te_mode                        0x00019eb5   Thumb Code   300  hal_internal_vsync.o(i.vsync_set_te_mode)
    .constdata                               0x0001a080   Section     8052  ap_demo.o(.constdata)
    g_cus_rx_dcs_execute_table               0x0001a080   Data         108  ap_demo.o(.constdata)
    .constdata                               0x0001bff4   Section      210  hal_gpio.o(.constdata)
    s_gpio_map                               0x0001bff4   Data         120  hal_gpio.o(.constdata)
    s_gpio_perf                              0x0001c06c   Data          90  hal_gpio.o(.constdata)
    .constdata                               0x0001c0c8   Section        8  drv_param_init.o(.constdata)
    .constdata                               0x0001c0d0   Section      390  drv_phy_common.o(.constdata)
    phy_para_mapping_h                       0x0001c0d0   Data         184  drv_phy_common.o(.constdata)
    phy_para_mapping_l                       0x0001c188   Data         128  drv_phy_common.o(.constdata)
    phy_data_high_map                        0x0001c208   Data          48  drv_phy_common.o(.constdata)
    phy_data_lp_map                          0x0001c238   Data          30  drv_phy_common.o(.constdata)
    .conststring                             0x0001c258   Section       72  hal_dsi_rx_ctrl.o(.conststring)
    .conststring                             0x0001c2a0   Section       67  hal_dsi_tx_ctrl.o(.conststring)
    .conststring                             0x0001c2e4   Section      376  hal_internal_vsync.o(.conststring)
    .ARM.__AT_0x00070100                     0x00070100   Section      192  irq_redirect .o(.ARM.__AT_0x00070100)
    .data                                    0x000701d0   Section      568  ap_demo.o(.data)
    start_display_on                         0x000701d0   Data           1  ap_demo.o(.data)
    g_exit_sleep_mode                        0x000701d1   Data           1  ap_demo.o(.data)
    S21_G991B_frame_update                   0x000701d2   Data           1  ap_demo.o(.data)
    s_in_aod_mode_flag                       0x000701d3   Data           1  ap_demo.o(.data)
    s_in_bule_mode_flag                      0x000701d4   Data           1  ap_demo.o(.data)
    panel_display_done                       0x000701d5   Data           1  ap_demo.o(.data)
    isStart                                  0x000701d6   Data           1  ap_demo.o(.data)
    flag_0a                                  0x000701d9   Data           1  ap_demo.o(.data)
    flag_5a                                  0x000701da   Data           1  ap_demo.o(.data)
    flag_c9_43                               0x000701db   Data           1  ap_demo.o(.data)
    ret_7f_count                             0x000701dc   Data           1  ap_demo.o(.data)
    ret_a1_count                             0x000701dd   Data           1  ap_demo.o(.data)
    ret_a2_count                             0x000701de   Data           1  ap_demo.o(.data)
    ret_c6_count                             0x000701df   Data           1  ap_demo.o(.data)
    ret_c7_count                             0x000701e0   Data           1  ap_demo.o(.data)
    ret_c8_count                             0x000701e1   Data           1  ap_demo.o(.data)
    ret_c9_count                             0x000701e2   Data           1  ap_demo.o(.data)
    frame_rate                               0x000701e3   Data           1  ap_demo.o(.data)
    Flag                                     0x000701e4   Data           1  ap_demo.o(.data)
    g_rx_ctrl_handle                         0x000701f0   Data           4  ap_demo.o(.data)
    g_tx_ctrl_handle                         0x000701f4   Data           4  ap_demo.o(.data)
    curFrame                                 0x000701f8   Data           4  ap_demo.o(.data)
    value_reg_df                             0x00070200   Data           4  ap_demo.o(.data)
    ExitDelay                                0x00070204   Data           4  ap_demo.o(.data)
    .data                                    0x00070408   Section       59  app_tp_st_touch.o(.data)
    s_calibration_flag                       0x0007040b   Data           1  app_tp_st_touch.o(.data)
    s_calibration_correct_flag               0x0007040c   Data           1  app_tp_st_touch.o(.data)
    .data                                    0x00070444   Section      228  app_tp_for_custom_s8.o(.data)
    app_tp_count                             0x0007044e   Data           1  app_tp_for_custom_s8.o(.data)
    phone_85_flag                            0x0007044f   Data           1  app_tp_for_custom_s8.o(.data)
    phone_F6_flag                            0x00070450   Data           1  app_tp_for_custom_s8.o(.data)
    phone_E4_flag                            0x00070451   Data           1  app_tp_for_custom_s8.o(.data)
    phone_72_flag                            0x00070452   Data           1  app_tp_for_custom_s8.o(.data)
    phone_75_flag                            0x00070453   Data           1  app_tp_for_custom_s8.o(.data)
    phone_92_flag                            0x00070454   Data           1  app_tp_for_custom_s8.o(.data)
    phone_74_flag                            0x00070455   Data           1  app_tp_for_custom_s8.o(.data)
    u16CoordY                                0x00070458   Data           2  app_tp_for_custom_s8.o(.data)
    u16CoordX                                0x0007045a   Data           2  app_tp_for_custom_s8.o(.data)
    u16CoordY_back                           0x0007045c   Data           2  app_tp_for_custom_s8.o(.data)
    u16CoordX_back                           0x0007045e   Data           2  app_tp_for_custom_s8.o(.data)
    .data                                    0x00070528   Section        8  hal_dsi_rx_ctrl.o(.data)
    g_hw_auto_filter                         0x00070528   Data           1  hal_dsi_rx_ctrl.o(.data)
    g_esc_clk                                0x0007052c   Data           4  hal_dsi_rx_ctrl.o(.data)
    .data                                    0x00070530   Section        3  hal_dsi_tx_ctrl.o(.data)
    g_tx_vcom_en                             0x00070530   Data           1  hal_dsi_tx_ctrl.o(.data)
    g_tx_vpg_en                              0x00070531   Data           1  hal_dsi_tx_ctrl.o(.data)
    g_tx_mode                                0x00070532   Data           1  hal_dsi_tx_ctrl.o(.data)
    .data                                    0x00070534   Section       24  hal_internal_vsync.o(.data)
    sg_cmd_mode_tx_start                     0x00070534   Data           1  hal_internal_vsync.o(.data)
    sg_cur_te_info                           0x00070538   Data           4  hal_internal_vsync.o(.data)
    g_cus_rx_write_cmd_handle                0x00070540   Data          12  hal_internal_vsync.o(.data)
    .data                                    0x0007054c   Section       12  drv_common.o(.data)
    s_my_tick                                0x0007054c   Data           4  drv_common.o(.data)
    .data                                    0x00070558   Section        4  drv_gpio.o(.data)
    g_ap_reset_cb                            0x00070558   Data           4  drv_gpio.o(.data)
    .data                                    0x0007055c   Section        4  drv_i2c_master.o(.data)
    i2c1_intr_callback                       0x0007055c   Data           4  drv_i2c_master.o(.data)
    .data                                    0x00070560   Section        4  drv_i2c_slave.o(.data)
    i2c0_intr_callback                       0x00070560   Data           4  drv_i2c_slave.o(.data)
    .data                                    0x00070564   Section     1188  drv_param_init.o(.data)
    .data                                    0x00070a08   Section        4  drv_spi_master.o(.data)
    SPIM_intr_callback                       0x00070a08   Data           4  drv_spi_master.o(.data)
    .data                                    0x00070a0c   Section        1  drv_sys_cfg.o(.data)
    sg_ap_rstn_trigger_type                  0x00070a0c   Data           1  drv_sys_cfg.o(.data)
    .data                                    0x00070a10   Section        8  drv_rxbr.o(.data)
    .data                                    0x00070a18   Section        4  drv_vidc.o(.data)
    .data                                    0x00070a1c   Section        1  drv_phy_common.o(.data)
    g_phy_calibration                        0x00070a1c   Data           1  drv_phy_common.o(.data)
    .data                                    0x00070a20   Section       12  drv_chip_info.o(.data)
    sg_chip_info                             0x00070a20   Data           4  drv_chip_info.o(.data)
    sg_chip_function                         0x00070a24   Data           4  drv_chip_info.o(.data)
    sg_chip_encrypt                          0x00070a28   Data           4  drv_chip_info.o(.data)
    .data                                    0x00070a2c   Section       18  norflash.o(.data)
    tmprg                                    0x00070a34   Data           4  norflash.o(.data)
    .data                                    0x00070a40   Section       12  drv_pwm.o(.data)
    s_pwm_type                               0x00070a40   Data           1  drv_pwm.o(.data)
    s_pwm_cb                                 0x00070a44   Data           8  drv_pwm.o(.data)
    .data                                    0x00070a4c   Section        8  drv_swire.o(.data)
    s_swire_cb                               0x00070a4c   Data           8  drv_swire.o(.data)
    .data                                    0x00070a54   Section       80  drv_timer.o(.data)
    sg_timer_info                            0x00070a54   Data          80  drv_timer.o(.data)
    .data                                    0x00070aa4   Section        8  drv_uart.o(.data)
    s_UartFcrReg                             0x00070aa4   Data           4  drv_uart.o(.data)
    uart_userData                            0x00070aa8   Data           4  drv_uart.o(.data)
    .data                                    0x00070aac   Section       12  drv_wdg.o(.data)
    sg_wdg_repeat                            0x00070aac   Data           1  drv_wdg.o(.data)
    sg_wdg_cb                                0x00070ab0   Data           8  drv_wdg.o(.data)
    .data                                    0x00070ab8   Section        4  stdout.o(.data)
    .data                                    0x00070abc   Section        4  errno.o(.data)
    _errno                                   0x00070abc   Data           4  errno.o(.data)
    .bss                                     0x00070ac0   Section       36  ap_demo.o(.bss)
    ccm                                      0x00070ac0   Data          36  ap_demo.o(.bss)
    .bss                                     0x00070ae4   Section      196  hal_dsi_rx_ctrl.o(.bss)
    g_rx_ctrl_handle_inst                    0x00070ae4   Data         196  hal_dsi_rx_ctrl.o(.bss)
    .bss                                     0x00070ba8   Section       76  hal_dsi_tx_ctrl.o(.bss)
    g_tx_ctrl_handle_inst                    0x00070ba8   Data          76  hal_dsi_tx_ctrl.o(.bss)
    .bss                                     0x00070bf4   Section      256  tau_log.o(.bss)
    .bss                                     0x00070cf4   Section      208  hal_uart.o(.bss)
    .bss                                     0x00070dc4   Section     2420  hal_internal_vsync.o(.bss)
    g_imm_buffer                             0x00071618   Data         255  hal_internal_vsync.o(.bss)
    sg_te_info                               0x00071718   Data          12  hal_internal_vsync.o(.bss)
    g_imm_packet                             0x00071724   Data          20  hal_internal_vsync.o(.bss)
    .bss                                     0x00071738   Section       28  drv_dma.o(.bss)
    s_dma_handle                             0x00071738   Data          28  drv_dma.o(.bss)
    .bss                                     0x00071754   Section       64  drv_gpio.o(.bss)
    s_gpio_cb                                0x00071754   Data          64  drv_gpio.o(.bss)
    .bss                                     0x00071794   Section       64  hal_internal_soft_sync.o(.bss)
    sg_sys_handler                           0x00071794   Data          64  hal_internal_soft_sync.o(.bss)
    .bss                                     0x000717d4   Section       32  hal_spi_slave.o(.bss)
    .bss                                     0x000717f4   Section     4144  dcs_packet_fifo.o(.bss)
    STACK                                    0x00072828   Section     4096  startup_armcm0.o(STACK)

    Global Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    BuildAttributes$$THM_ISAv3M$S$PE$A:L22$X:L11$S22$IEEE1$IW$USESV6$~STKCKD$USESV7$~SHL$OTIME$ROPI$IEEEJ$EBA8$MICROLIB$REQ8$PRES8$EABIv2 0x00000000   Number         0  anon$$obj.o ABSOLUTE
    __ARM_use_no_argv                        0x00000000   Number         0  main.o ABSOLUTE
    _printf_a                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_c                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_charcount                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_d                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_e                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_f                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_flags                            0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_dec                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_hex                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_g                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_i                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_int_dec                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_l                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ll                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lld                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lli                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llo                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llu                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llx                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_dec                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_hex                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_oct                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ls                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_mbtowc                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_n                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_o                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_p                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_percent                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_pre_padding                      0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_return_value                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_s                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_sizespec                         0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_str                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_signed                  0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_unsigned                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_u                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wctomb                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_widthprec                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_x                                0x00000000   Number         0  stubs.o ABSOLUTE
    __cpp_initialize__aeabi_                  - Undefined Weak Reference
    __cxa_finalize                            - Undefined Weak Reference
    _clock_init                               - Undefined Weak Reference
    _microlib_exit                            - Undefined Weak Reference
    __Vectors_Size                           0x000000c0   Number         0  startup_armcm0.o ABSOLUTE
    __Vectors                                0x00010000   Data           4  startup_armcm0.o(RESET)
    __Vectors_End                            0x000100c0   Data           0  startup_armcm0.o(RESET)
    __main                                   0x000100c1   Thumb Code     0  entry.o(.ARM.Collect$$$$00000000)
    _main_stk                                0x000100c1   Thumb Code     0  entry2.o(.ARM.Collect$$$$00000001)
    _main_scatterload                        0x000100c5   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    __main_after_scatterload                 0x000100c9   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    _main_clock                              0x000100c9   Thumb Code     0  entry7b.o(.ARM.Collect$$$$00000008)
    _main_cpp_init                           0x000100c9   Thumb Code     0  entry8b.o(.ARM.Collect$$$$0000000A)
    _main_init                               0x000100c9   Thumb Code     0  entry9a.o(.ARM.Collect$$$$0000000B)
    __rt_final_cpp                           0x000100d1   Thumb Code     0  entry10a.o(.ARM.Collect$$$$0000000D)
    __rt_final_exit                          0x000100d1   Thumb Code     0  entry11a.o(.ARM.Collect$$$$0000000F)
    Reset_Handler                            0x000100d5   Thumb Code    28  startup_armcm0.o(.text)
    NMI_Handler                              0x000100f1   Thumb Code     2  startup_armcm0.o(.text)
    SVC_Handler                              0x000100f5   Thumb Code     2  startup_armcm0.o(.text)
    PendSV_Handler                           0x000100f7   Thumb Code     2  startup_armcm0.o(.text)
    OTP_IRQn_Handler                         0x00010123   Thumb Code     2  startup_armcm0.o(.text)
    PVD_IRQn_Handler                         0x00010127   Thumb Code     2  startup_armcm0.o(.text)
    __aeabi_uidiv                            0x0001014d   Thumb Code     0  uidiv.o(.text)
    __aeabi_uidivmod                         0x0001014d   Thumb Code    44  uidiv.o(.text)
    __aeabi_idiv                             0x00010179   Thumb Code     0  idiv.o(.text)
    __aeabi_idivmod                          0x00010179   Thumb Code    40  idiv.o(.text)
    __aeabi_memcpy                           0x000101a1   Thumb Code    36  memcpya.o(.text)
    __aeabi_memcpy4                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memcpy8                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memset                           0x000101c5   Thumb Code    14  memseta.o(.text)
    __aeabi_memset4                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memset8                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr                           0x000101d3   Thumb Code     4  memseta.o(.text)
    __aeabi_memclr4                          0x000101d3   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr8                          0x000101d3   Thumb Code     0  memseta.o(.text)
    _memset$wrapper                          0x000101d7   Thumb Code    18  memseta.o(.text)
    __aeabi_fadd                             0x000101e9   Thumb Code   162  fadd.o(.text)
    __aeabi_fsub                             0x0001028b   Thumb Code     8  fadd.o(.text)
    __aeabi_frsub                            0x00010293   Thumb Code     8  fadd.o(.text)
    __aeabi_fmul                             0x0001029b   Thumb Code   122  fmul.o(.text)
    __aeabi_fdiv                             0x00010315   Thumb Code   124  fdiv.o(.text)
    __ARM_scalbnf                            0x00010391   Thumb Code    24  fscalb.o(.text)
    scalbnf                                  0x00010391   Thumb Code     0  fscalb.o(.text)
    __aeabi_dadd                             0x000103a9   Thumb Code   328  dadd.o(.text)
    __aeabi_dsub                             0x000104f1   Thumb Code    12  dadd.o(.text)
    __aeabi_drsub                            0x000104fd   Thumb Code    12  dadd.o(.text)
    __aeabi_dmul                             0x0001050d   Thumb Code   202  dmul.o(.text)
    __aeabi_ddiv                             0x000105dd   Thumb Code   234  ddiv.o(.text)
    __aeabi_i2f                              0x000106cd   Thumb Code    22  fflti.o(.text)
    __aeabi_ui2f                             0x000106e3   Thumb Code    14  ffltui.o(.text)
    __aeabi_ui2d                             0x000106f1   Thumb Code    24  dfltui.o(.text)
    __aeabi_f2iz                             0x0001070d   Thumb Code    50  ffixi.o(.text)
    __aeabi_f2uiz                            0x0001073f   Thumb Code    40  ffixui.o(.text)
    __aeabi_d2iz                             0x00010769   Thumb Code    62  dfixi.o(.text)
    __aeabi_d2uiz                            0x000107b1   Thumb Code    50  dfixui.o(.text)
    __aeabi_f2d                              0x000107ed   Thumb Code    40  f2d.o(.text)
    __aeabi_cdcmpeq                          0x00010815   Thumb Code     0  cdcmple.o(.text)
    __aeabi_cdcmple                          0x00010815   Thumb Code    38  cdcmple.o(.text)
    __aeabi_cfcmpeq                          0x0001083d   Thumb Code     0  cfcmple.o(.text)
    __aeabi_cfcmple                          0x0001083d   Thumb Code    20  cfcmple.o(.text)
    __aeabi_cfrcmple                         0x00010851   Thumb Code    20  cfrcmple.o(.text)
    __aeabi_uldivmod                         0x00010865   Thumb Code    96  uldiv.o(.text)
    __aeabi_llsl                             0x000108c5   Thumb Code    32  llshl.o(.text)
    _ll_shift_l                              0x000108c5   Thumb Code     0  llshl.o(.text)
    __aeabi_llsr                             0x000108e5   Thumb Code    34  llushr.o(.text)
    _ll_ushift_r                             0x000108e5   Thumb Code     0  llushr.o(.text)
    __aeabi_lasr                             0x00010907   Thumb Code    38  llsshr.o(.text)
    _ll_sshift_r                             0x00010907   Thumb Code     0  llsshr.o(.text)
    __I$use$fp                               0x0001092d   Thumb Code     0  iusefp.o(.text)
    _float_round                             0x0001092d   Thumb Code    16  fepilogue.o(.text)
    _float_epilogue                          0x0001093d   Thumb Code   114  fepilogue.o(.text)
    _double_round                            0x000109af   Thumb Code    26  depilogue.o(.text)
    _double_epilogue                         0x000109c9   Thumb Code   164  depilogue.o(.text)
    _dsqrt                                   0x00010a6d   Thumb Code   162  dsqrt.o(.text)
    __aeabi_d2ulz                            0x00010b11   Thumb Code    54  dfixul.o(.text)
    __aeabi_cdrcmple                         0x00010b51   Thumb Code    38  cdrcmple.o(.text)
    __scatterload                            0x00010b79   Thumb Code    28  init.o(.text)
    __scatterload_rt2                        0x00010b79   Thumb Code     0  init.o(.text)
    __decompress                             0x00010b9d   Thumb Code     0  __dczerorl2.o(.text)
    __decompress1                            0x00010b9d   Thumb Code    86  __dczerorl2.o(.text)
    ADC_IRQn_Handler                         0x00010bf5   Thumb Code    18  irq_redirect .o(i.ADC_IRQn_Handler)
    AP_NRESET_IRQn_Handler                   0x00010c0d   Thumb Code    18  irq_redirect .o(i.AP_NRESET_IRQn_Handler)
    DMA_IRQn_Handler                         0x00010c25   Thumb Code    14  irq_redirect .o(i.DMA_IRQn_Handler)
    EXTI_INT0_IRQn_Handler                   0x00010c39   Thumb Code    22  irq_redirect .o(i.EXTI_INT0_IRQn_Handler)
    EXTI_INT1_IRQn_Handler                   0x00010c55   Thumb Code    22  irq_redirect .o(i.EXTI_INT1_IRQn_Handler)
    EXTI_INT2_IRQn_Handler                   0x00010c71   Thumb Code    22  irq_redirect .o(i.EXTI_INT2_IRQn_Handler)
    EXTI_INT3_IRQn_Handler                   0x00010c8d   Thumb Code    22  irq_redirect .o(i.EXTI_INT3_IRQn_Handler)
    EXTI_INT4_IRQn_Handler                   0x00010ca9   Thumb Code    22  irq_redirect .o(i.EXTI_INT4_IRQn_Handler)
    EXTI_INT5_IRQn_Handler                   0x00010cc5   Thumb Code    22  irq_redirect .o(i.EXTI_INT5_IRQn_Handler)
    EXTI_INT6_IRQn_Handler                   0x00010ce1   Thumb Code    22  irq_redirect .o(i.EXTI_INT6_IRQn_Handler)
    EXTI_INT7_IRQn_Handler                   0x00010cfd   Thumb Code    22  irq_redirect .o(i.EXTI_INT7_IRQn_Handler)
    FLSCTRL_IRQn_Handler                     0x00010d19   Thumb Code    14  irq_redirect .o(i.FLSCTRL_IRQn_Handler)
    Gpio_swire_output                        0x00010d2d   Thumb Code    78  ap_demo.o(i.Gpio_swire_output)
    HardFault_Handler                        0x00010d7d   Thumb Code    14  irq_redirect .o(i.HardFault_Handler)
    I2C0_IRQn_Handler                        0x00010d91   Thumb Code    18  irq_redirect .o(i.I2C0_IRQn_Handler)
    I2C1_IRQn_Handler                        0x00010da9   Thumb Code    18  irq_redirect .o(i.I2C1_IRQn_Handler)
    LCDC_IRQn_Handler                        0x00010dc1   Thumb Code    18  irq_redirect .o(i.LCDC_IRQn_Handler)
    LOG_printf                               0x00010dd9   Thumb Code    30  tau_log.o(i.LOG_printf)
    MEMC_IRQn_Handler                        0x00010e01   Thumb Code    18  irq_redirect .o(i.MEMC_IRQn_Handler)
    MIPI_RX_IRQn_Handler                     0x00010e19   Thumb Code    18  irq_redirect .o(i.MIPI_RX_IRQn_Handler)
    MIPI_TX_IRQn_Handler                     0x00010e31   Thumb Code    18  irq_redirect .o(i.MIPI_TX_IRQn_Handler)
    PWMDET_IRQn_Handler                      0x00010e49   Thumb Code    22  irq_redirect .o(i.PWMDET_IRQn_Handler)
    SPIM_IRQn_Handler                        0x00010f29   Thumb Code    22  irq_redirect .o(i.SPIM_IRQn_Handler)
    SPIS_IRQn_Handler                        0x00010f45   Thumb Code    22  irq_redirect .o(i.SPIS_IRQn_Handler)
    SWIRE_IRQn_Handler                       0x00010f61   Thumb Code    22  irq_redirect .o(i.SWIRE_IRQn_Handler)
    SysTick_Handler                          0x00010f7d   Thumb Code    18  irq_redirect .o(i.SysTick_Handler)
    TIMER0_IRQn_Handler                      0x00010f95   Thumb Code    18  irq_redirect .o(i.TIMER0_IRQn_Handler)
    TIMER1_IRQn_Handler                      0x00010fad   Thumb Code    18  irq_redirect .o(i.TIMER1_IRQn_Handler)
    TIMER2_IRQn_Handler                      0x00010fc5   Thumb Code    18  irq_redirect .o(i.TIMER2_IRQn_Handler)
    TIMER3_IRQn_Handler                      0x00010fdd   Thumb Code    18  irq_redirect .o(i.TIMER3_IRQn_Handler)
    UART_DisableDma                          0x00010ff5   Thumb Code     2  drv_uart.o(i.UART_DisableDma)
    UART_GetInstance                         0x00010ff7   Thumb Code     4  drv_uart.o(i.UART_GetInstance)
    __scatterload_null                       0x00010ffb   Thumb Code     2  handlers.o(i.__scatterload_null)
    drv_dsi_rx_set_inten                     0x00010ffd   Thumb Code     4  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    s_RAM_CK                                 0x00011000   Data          20  drv_common.o(.ARM.__at_0x11000)
    drv_dsi_tx_command_put_payload           0x00011015   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    s_debug_state                            0x00011018   Data           4  drv_common.o(.ARM.__at_0x11018)
    UART0_IRQ_Handle                         0x0001101d   Thumb Code    20  drv_uart.o(i.UART0_IRQ_Handle)
    UART_IRQn_Handler                        0x00011039   Thumb Code    18  irq_redirect .o(i.UART_IRQn_Handler)
    UART_ResetRxFIFO                         0x00011051   Thumb Code    32  drv_uart.o(i.UART_ResetRxFIFO)
    UART_SetBaudRate                         0x00011075   Thumb Code    72  drv_uart.o(i.UART_SetBaudRate)
    UART_SwitchSCLK                          0x000110bd   Thumb Code    26  drv_uart.o(i.UART_SwitchSCLK)
    UART_TransferHandleIRQ                   0x000110d7   Thumb Code   308  drv_uart.o(i.UART_TransferHandleIRQ)
    UART_WriteBlocking                       0x0001120b   Thumb Code    26  drv_uart.o(i.UART_WriteBlocking)
    UART_init                                0x00011225   Thumb Code   182  drv_uart.o(i.UART_init)
    VIDC_IRQn_Handler                        0x000112e1   Thumb Code    18  irq_redirect .o(i.VIDC_IRQn_Handler)
    VPRE_IRQn_Handler                        0x000112f9   Thumb Code    18  irq_redirect .o(i.VPRE_IRQn_Handler)
    WDG_IRQn_Handler                         0x00011311   Thumb Code    18  irq_redirect .o(i.WDG_IRQn_Handler)
    __0printf                                0x00011329   Thumb Code    24  printfa.o(i.__0printf)
    __1printf                                0x00011329   Thumb Code     0  printfa.o(i.__0printf)
    __2printf                                0x00011329   Thumb Code     0  printfa.o(i.__0printf)
    __c89printf                              0x00011329   Thumb Code     0  printfa.o(i.__0printf)
    printf                                   0x00011329   Thumb Code     0  printfa.o(i.__0printf)
    __0vsprintf                              0x00011349   Thumb Code    30  printfa.o(i.__0vsprintf)
    __1vsprintf                              0x00011349   Thumb Code     0  printfa.o(i.__0vsprintf)
    __2vsprintf                              0x00011349   Thumb Code     0  printfa.o(i.__0vsprintf)
    __c89vsprintf                            0x00011349   Thumb Code     0  printfa.o(i.__0vsprintf)
    vsprintf                                 0x00011349   Thumb Code     0  printfa.o(i.__0vsprintf)
    __ARM_clz                                0x0001136d   Thumb Code    46  depilogue.o(i.__ARM_clz)
    __ARM_common_switch8                     0x0001139b   Thumb Code    26  hal_dsi_rx_ctrl.o(i.__ARM_common_switch8)
    __scatterload_copy                       0x00011449   Thumb Code    14  handlers.o(i.__scatterload_copy)
    __scatterload_zeroinit                   0x00011457   Thumb Code    14  handlers.o(i.__scatterload_zeroinit)
    __set_errno                              0x00011465   Thumb Code     6  errno.o(i.__set_errno)
    ap_demo                                  0x00012da1   Thumb Code   234  ap_demo.o(i.ap_demo)
    ap_get_tp_calibration_status_01          0x00012f11   Thumb Code    28  app_tp_st_touch.o(i.ap_get_tp_calibration_status_01)
    app_ADC_IRQn_Handler                     0x00013169   Thumb Code    22  drv_rxbr.o(i.app_ADC_IRQn_Handler)
    app_AP_NRESET_IRQn_Handler               0x00013185   Thumb Code    32  drv_gpio.o(i.app_AP_NRESET_IRQn_Handler)
    app_EXTI_INT0_IRQn_Handler               0x000131a9   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT0_IRQn_Handler)
    app_EXTI_INT1_IRQn_Handler               0x000131c5   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT1_IRQn_Handler)
    app_EXTI_INT2_IRQn_Handler               0x000131e1   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT2_IRQn_Handler)
    app_EXTI_INT3_IRQn_Handler               0x000131fd   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT3_IRQn_Handler)
    app_EXTI_INT4_IRQn_Handler               0x00013219   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT4_IRQn_Handler)
    app_EXTI_INT5_IRQn_Handler               0x00013235   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT5_IRQn_Handler)
    app_EXTI_INT6_IRQn_Handler               0x00013251   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT6_IRQn_Handler)
    app_EXTI_INT7_IRQn_Handler               0x0001326d   Thumb Code    22  drv_gpio.o(i.app_EXTI_INT7_IRQn_Handler)
    app_HardFault_Handler                    0x00013289   Thumb Code    12  drv_common.o(i.app_HardFault_Handler)
    app_I2C0_IRQn_Handler                    0x000132d1   Thumb Code    14  drv_i2c_slave.o(i.app_I2C0_IRQn_Handler)
    app_I2C1_IRQn_Handler                    0x000132e9   Thumb Code     8  drv_i2c_master.o(i.app_I2C1_IRQn_Handler)
    app_LCDC_IRQn_Handler                    0x000132f9   Thumb Code   146  hal_internal_vsync.o(i.app_LCDC_IRQn_Handler)
    app_MEMC_IRQn_Handler                    0x00013429   Thumb Code   132  drv_memc.o(i.app_MEMC_IRQn_Handler)
    app_MIPI_RX_IRQn_Handler                 0x000134b1   Thumb Code   232  drv_dsi_rx.o(i.app_MIPI_RX_IRQn_Handler)
    app_MIPI_TX_IRQn_Handler                 0x00013749   Thumb Code    56  drv_dsi_tx.o(i.app_MIPI_TX_IRQn_Handler)
    app_PWMDET_IRQn_Handler                  0x000137e9   Thumb Code    62  drv_pwm.o(i.app_PWMDET_IRQn_Handler)
    app_SPIM_IRQn_Handler                    0x00013831   Thumb Code    34  drv_spi_master.o(i.app_SPIM_IRQn_Handler)
    app_SPIS_IRQn_Handler                    0x00013861   Thumb Code   500  hal_spi_slave.o(i.app_SPIS_IRQn_Handler)
    app_SWIRE_IRQn_Handler                   0x00013a61   Thumb Code    28  drv_swire.o(i.app_SWIRE_IRQn_Handler)
    app_SysTick_Handler                      0x00013a81   Thumb Code    20  drv_common.o(i.app_SysTick_Handler)
    app_TIMER0_IRQn_Handler                  0x00013a99   Thumb Code    10  drv_timer.o(i.app_TIMER0_IRQn_Handler)
    app_TIMER1_IRQn_Handler                  0x00013aa3   Thumb Code    10  drv_timer.o(i.app_TIMER1_IRQn_Handler)
    app_TIMER2_IRQn_Handler                  0x00013aad   Thumb Code    10  drv_timer.o(i.app_TIMER2_IRQn_Handler)
    app_TIMER3_IRQn_Handler                  0x00013ab7   Thumb Code    10  drv_timer.o(i.app_TIMER3_IRQn_Handler)
    app_UART_IRQn_Handler                    0x00013ac1   Thumb Code     8  drv_uart.o(i.app_UART_IRQn_Handler)
    app_VIDC_IRQn_Handler                    0x00013ac9   Thumb Code    22  drv_vidc.o(i.app_VIDC_IRQn_Handler)
    app_VPRE_IRQn_Handler                    0x00013ae5   Thumb Code    22  drv_rxbr.o(i.app_VPRE_IRQn_Handler)
    app_WDG_IRQn_Handler                     0x00013b01   Thumb Code    52  drv_wdg.o(i.app_WDG_IRQn_Handler)
    app_dma_irq_handler                      0x00013b39   Thumb Code    10  drv_dma.o(i.app_dma_irq_handler)
    app_fls_ctrl_Handler                     0x00013b49   Thumb Code    38  norflash.o(i.app_fls_ctrl_Handler)
    board_Init                               0x00013b79   Thumb Code    30  board.o(i.board_Init)
    calc_framebuffer_setting                 0x00013b9d   Thumb Code  1416  hal_internal_vsync.o(i.calc_framebuffer_setting)
    ceil                                     0x00014129   Thumb Code   180  ceil.o(i.ceil)
    dcs_packet_fifo_alloc                    0x000142a1   Thumb Code    80  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    dcs_packet_fifo_init                     0x000142f9   Thumb Code    18  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    dcs_packet_free_fifo_header              0x00014311   Thumb Code    60  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    dcs_packet_get_fifo_header               0x00014355   Thumb Code    26  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    delayMs                                  0x000143a5   Thumb Code    24  tau_delay.o(i.delayMs)
    delayUs                                  0x000143bd   Thumb Code    34  tau_delay.o(i.delayUs)
    drv_ap_rst_trig_edge_detect              0x000143e1   Thumb Code    46  drv_sys_cfg.o(i.drv_ap_rst_trig_edge_detect)
    drv_chip_info_get_info                   0x00014419   Thumb Code     6  drv_chip_info.o(i.drv_chip_info_get_info)
    drv_chip_info_init                       0x00014425   Thumb Code    56  drv_chip_info.o(i.drv_chip_info_init)
    drv_chip_rx_info_check                   0x00014465   Thumb Code    98  drv_chip_info.o(i.drv_chip_rx_info_check)
    drv_chip_rx_init_done                    0x00014515   Thumb Code    16  drv_chip_info.o(i.drv_chip_rx_init_done)
    drv_common_enable_systick                0x00014529   Thumb Code    70  drv_common.o(i.drv_common_enable_systick)
    drv_common_get_tick                      0x00014581   Thumb Code     6  drv_common.o(i.drv_common_get_tick)
    drv_common_system_init                   0x0001458d   Thumb Code     8  drv_common.o(i.drv_common_system_init)
    drv_crgu_config_reset_modules            0x00014595   Thumb Code    10  drv_crgu.o(i.drv_crgu_config_reset_modules)
    drv_crgu_set_ahb_pre_div                 0x000145a5   Thumb Code    14  drv_crgu.o(i.drv_crgu_set_ahb_pre_div)
    drv_crgu_set_ahb_src                     0x000145b9   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_ahb_src)
    drv_crgu_set_clock                       0x000145cd   Thumb Code    26  drv_crgu.o(i.drv_crgu_set_clock)
    drv_crgu_set_dpi_mux_src                 0x000145ed   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dpi_mux_src)
    drv_crgu_set_dpi_pre_div                 0x00014601   Thumb Code    18  drv_crgu.o(i.drv_crgu_set_dpi_pre_div)
    drv_crgu_set_dpi_pre_src                 0x00014619   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dpi_pre_src)
    drv_crgu_set_dsc_core_div                0x0001462d   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dsc_core_div)
    drv_crgu_set_dsco_src                    0x00014641   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dsco_src)
    drv_crgu_set_dsco_src_div                0x00014655   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_dsco_src_div)
    drv_crgu_set_fb_div                      0x00014669   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_fb_div)
    drv_crgu_set_fb_src                      0x0001467d   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_fb_src)
    drv_crgu_set_lcdc_div                    0x00014691   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_lcdc_div)
    drv_crgu_set_lcdc_src                    0x000146a5   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_lcdc_src)
    drv_crgu_set_mipi_cfg_src                0x000146b9   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_mipi_cfg_src)
    drv_crgu_set_mipi_ref_src                0x000146cd   Thumb Code    18  drv_crgu.o(i.drv_crgu_set_mipi_ref_src)
    drv_crgu_set_reset                       0x000146e5   Thumb Code    20  drv_crgu.o(i.drv_crgu_set_reset)
    drv_crgu_set_rxbr_div                    0x000146fd   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_rxbr_div)
    drv_crgu_set_rxbr_src                    0x00014711   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_rxbr_src)
    drv_crgu_set_vidc_src                    0x00014725   Thumb Code    16  drv_crgu.o(i.drv_crgu_set_vidc_src)
    drv_dma_clear_flag                       0x00014739   Thumb Code    24  drv_dma.o(i.drv_dma_clear_flag)
    drv_dma_get_channel_flag                 0x00014751   Thumb Code    12  drv_dma.o(i.drv_dma_get_channel_flag)
    drv_dma_irq_handler                      0x0001475d   Thumb Code   138  drv_dma.o(i.drv_dma_irq_handler)
    drv_dsc_dec_convert_pps_rc_parameter     0x000147ed   Thumb Code    54  drv_dsc_dec.o(i.drv_dsc_dec_convert_pps_rc_parameter)
    drv_dsc_dec_disable                      0x00014823   Thumb Code    12  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    drv_dsc_dec_enable                       0x00014831   Thumb Code    88  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    drv_dsc_dec_get_nslc                     0x000148a5   Thumb Code    10  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    drv_dsc_dec_set_u8_pps                   0x000148af   Thumb Code    40  drv_dsc_dec.o(i.drv_dsc_dec_set_u8_pps)
    drv_dsi_rx_calc_ipi_tx_delay             0x000148d9   Thumb Code   244  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    drv_dsi_rx_enable_irq                    0x000149dd   Thumb Code    58  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    drv_dsi_rx_get_bta_status                0x00014a1d   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_get_bta_status)
    drv_dsi_rx_get_compression_en            0x00014a99   Thumb Code     8  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    drv_dsi_rx_get_max_ret_size              0x00014aa1   Thumb Code     6  drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size)
    drv_dsi_rx_power_up                      0x00014aa7   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    drv_dsi_rx_set_ctrl_cfg                  0x00014ab5   Thumb Code    32  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    drv_dsi_rx_set_ddi_cfg                   0x00014ad5   Thumb Code    16  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    drv_dsi_rx_set_ipi_cfg                   0x00014ae5   Thumb Code    16  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    drv_dsi_rx_set_lane_swap                 0x00014af5   Thumb Code    70  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    drv_dsi_rx_set_resp_cnt                  0x00014b3b   Thumb Code    38  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    drv_dsi_rx_set_up_phy                    0x00014b61   Thumb Code   256  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    drv_dsi_rx_shut_down                     0x00014c65   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    drv_dsi_tx_command_header                0x00014c73   Thumb Code    20  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    drv_dsi_tx_command_mode_cfg              0x00014c87   Thumb Code   108  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    drv_dsi_tx_config_eotp                   0x00014cf3   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    drv_dsi_tx_config_int                    0x00014d0b   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    drv_dsi_tx_dpi_lpcmd_time                0x00014d13   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    drv_dsi_tx_dpi_mode                      0x00014d1b   Thumb Code    10  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    drv_dsi_tx_dpi_polarity                  0x00014d25   Thumb Code    36  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    drv_dsi_tx_edpi_cmd_size                 0x00014d49   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    drv_dsi_tx_get_cmd_status                0x00014d4d   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    drv_dsi_tx_mode                          0x00014d51   Thumb Code     4  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    drv_dsi_tx_phy_clock_lane_auto_lp        0x00014d55   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    drv_dsi_tx_phy_clock_lane_req_hs         0x00014d6d   Thumb Code    26  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    drv_dsi_tx_phy_lane_mode                 0x00014d87   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    drv_dsi_tx_phy_status_ready              0x00014d93   Thumb Code   100  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    drv_dsi_tx_phy_status_stopstate          0x00014df7   Thumb Code    62  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    drv_dsi_tx_phy_test_setup                0x00014e35   Thumb Code   308  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    drv_dsi_tx_phy_time_cfg                  0x00014f69   Thumb Code    30  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    drv_dsi_tx_powerup                       0x00014f87   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    drv_dsi_tx_response_mode                 0x00014f8f   Thumb Code    28  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    drv_dsi_tx_set_bta_ack                   0x00014fab   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    drv_dsi_tx_set_esc_div                   0x00014fc3   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    drv_dsi_tx_set_int                       0x00014fd1   Thumb Code    58  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    drv_dsi_tx_set_time_out_div              0x00015011   Thumb Code    16  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    drv_dsi_tx_set_video_chunk               0x00015021   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    drv_dsi_tx_set_video_timing              0x00015029   Thumb Code    34  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    drv_dsi_tx_shutdown                      0x0001504b   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    drv_dsi_tx_timeout_cfg                   0x00015053   Thumb Code    38  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    drv_dsi_tx_video_mode_cfg                0x00015079   Thumb Code   170  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    drv_dsi_tx_video_mode_disable_hact_cmd   0x00015123   Thumb Code    22  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_disable_hact_cmd)
    drv_dsi_tx_video_mode_set_lp_cmd         0x00015139   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_set_lp_cmd)
    drv_efuse_enter_inactive                 0x00015151   Thumb Code    46  drv_efuse.o(i.drv_efuse_enter_inactive)
    drv_efuse_int_enable                     0x0001517f   Thumb Code    12  drv_efuse.o(i.drv_efuse_int_enable)
    drv_efuse_read                           0x0001518b   Thumb Code    50  drv_efuse.o(i.drv_efuse_read)
    drv_efuse_read_req                       0x000151bd   Thumb Code    24  drv_efuse.o(i.drv_efuse_read_req)
    drv_gpio_get_input_data                  0x000151d5   Thumb Code    20  drv_gpio.o(i.drv_gpio_get_input_data)
    drv_gpio_set_ioe                         0x000151ed   Thumb Code    26  drv_gpio.o(i.drv_gpio_set_ioe)
    drv_gpio_set_mode0                       0x0001520d   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode0)
    drv_gpio_set_mode1                       0x0001521d   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode1)
    drv_gpio_set_mode2                       0x0001522d   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode2)
    drv_gpio_set_mode3                       0x0001523d   Thumb Code    12  drv_gpio.o(i.drv_gpio_set_mode3)
    drv_gpio_set_pull_state                  0x0001526d   Thumb Code   298  drv_gpio.o(i.drv_gpio_set_pull_state)
    drv_lcdc_config_bypass                   0x0001539d   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_config_bypass)
    drv_lcdc_config_ccm                      0x000153b5   Thumb Code    48  drv_lcdc.o(i.drv_lcdc_config_ccm)
    drv_lcdc_config_disp_mode                0x000153e5   Thumb Code    22  drv_lcdc.o(i.drv_lcdc_config_disp_mode)
    drv_lcdc_config_dpi_polarity             0x000153fb   Thumb Code    36  drv_lcdc.o(i.drv_lcdc_config_dpi_polarity)
    drv_lcdc_config_dpi_timing               0x0001541f   Thumb Code    38  drv_lcdc.o(i.drv_lcdc_config_dpi_timing)
    drv_lcdc_config_edpi_mode                0x00015445   Thumb Code    22  drv_lcdc.o(i.drv_lcdc_config_edpi_mode)
    drv_lcdc_config_endianness               0x0001545b   Thumb Code    22  drv_lcdc.o(i.drv_lcdc_config_endianness)
    drv_lcdc_config_input_size               0x00015471   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_config_input_size)
    drv_lcdc_config_int                      0x0001547d   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_config_int)
    drv_lcdc_config_int_single               0x0001549b   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_int_single)
    drv_lcdc_config_overwrite                0x000154bd   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_overwrite)
    drv_lcdc_config_overwrite_rgb            0x000154df   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    drv_lcdc_config_partial_display_area     0x000154eb   Thumb Code    26  drv_lcdc.o(i.drv_lcdc_config_partial_display_area)
    drv_lcdc_config_partial_display_enable   0x00015505   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_partial_display_enable)
    drv_lcdc_config_scale_up_coef            0x00015527   Thumb Code    26  drv_lcdc.o(i.drv_lcdc_config_scale_up_coef)
    drv_lcdc_config_scale_up_step            0x00015541   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_config_scale_up_step)
    drv_lcdc_config_src_parameter            0x0001554d   Thumb Code    76  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    drv_lcdc_config_thresh                   0x00015599   Thumb Code     6  drv_lcdc.o(i.drv_lcdc_config_thresh)
    drv_lcdc_ctrl_flow                       0x0001559f   Thumb Code    18  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    drv_lcdc_enable_shadow_reg               0x000155b1   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    drv_lcdc_set_int                         0x000155d1   Thumb Code    58  drv_lcdc.o(i.drv_lcdc_set_int)
    drv_lcdc_set_prefetch                    0x00015611   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_set_prefetch)
    drv_lcdc_set_video_hw_mode               0x00015629   Thumb Code    20  drv_lcdc.o(i.drv_lcdc_set_video_hw_mode)
    drv_lcdc_start                           0x0001563d   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_start)
    drv_memc_clear_status                    0x0001565d   Thumb Code    12  drv_memc.o(i.drv_memc_clear_status)
    drv_memc_enable_irq                      0x00015669   Thumb Code    58  drv_memc.o(i.drv_memc_enable_irq)
    drv_memc_gen_a_tear_signal               0x000156a9   Thumb Code    12  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    drv_memc_get_status                      0x000156b5   Thumb Code    18  drv_memc.o(i.drv_memc_get_status)
    drv_memc_rate_transfer_sel               0x000156c7   Thumb Code    16  drv_memc.o(i.drv_memc_rate_transfer_sel)
    drv_memc_sel_vsync                       0x000156d7   Thumb Code    14  drv_memc.o(i.drv_memc_sel_vsync)
    drv_memc_set_active_height               0x000156e5   Thumb Code    14  drv_memc.o(i.drv_memc_set_active_height)
    drv_memc_set_data_mode                   0x000156f9   Thumb Code    12  drv_memc.o(i.drv_memc_set_data_mode)
    drv_memc_set_double_buffer               0x00015705   Thumb Code    16  drv_memc.o(i.drv_memc_set_double_buffer)
    drv_memc_set_double_buffer_reverse       0x00015715   Thumb Code    18  drv_memc.o(i.drv_memc_set_double_buffer_reverse)
    drv_memc_set_fs_en_conditions            0x00015727   Thumb Code    16  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    drv_memc_set_inten                       0x00015737   Thumb Code    20  drv_memc.o(i.drv_memc_set_inten)
    drv_memc_set_lcdc_st_conditions          0x0001574d   Thumb Code    18  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    drv_memc_set_ltpo_mode                   0x00015765   Thumb Code    26  drv_memc.o(i.drv_memc_set_ltpo_mode)
    drv_memc_set_tear_mode                   0x0001577f   Thumb Code    14  drv_memc.o(i.drv_memc_set_tear_mode)
    drv_memc_set_tear_waveform               0x0001578d   Thumb Code    34  drv_memc.o(i.drv_memc_set_tear_waveform)
    drv_memc_set_vidc_sync_cnt               0x000157b5   Thumb Code    14  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    drv_param_init_get_ccm                   0x000157c5   Thumb Code     4  drv_param_init.o(i.drv_param_init_get_ccm)
    drv_param_init_get_scld_filter_h         0x000157cd   Thumb Code    12  drv_param_init.o(i.drv_param_init_get_scld_filter_h)
    drv_param_init_get_scld_filter_v         0x000157e1   Thumb Code    12  drv_param_init.o(i.drv_param_init_get_scld_filter_v)
    drv_param_init_get_sclu_filter           0x000157f5   Thumb Code     4  drv_param_init.o(i.drv_param_init_get_sclu_filter)
    drv_param_init_set_ccm                   0x000157fd   Thumb Code    14  drv_param_init.o(i.drv_param_init_set_ccm)
    drv_param_init_set_scld_filter           0x00015811   Thumb Code    92  drv_param_init.o(i.drv_param_init_set_scld_filter)
    drv_param_p2r_filter_init                0x00015875   Thumb Code    30  drv_param_init.o(i.drv_param_p2r_filter_init)
    drv_phy_enable_calibration               0x00015899   Thumb Code    12  drv_phy_common.o(i.drv_phy_enable_calibration)
    drv_phy_get_calibration                  0x000158a9   Thumb Code    50  drv_phy_common.o(i.drv_phy_get_calibration)
    drv_phy_get_pll_para                     0x000158e5   Thumb Code    88  drv_phy_common.o(i.drv_phy_get_pll_para)
    drv_phy_get_rate_para                    0x00015945   Thumb Code    76  drv_phy_common.o(i.drv_phy_get_rate_para)
    drv_phy_test_clear                       0x00015999   Thumb Code    16  drv_phy_common.o(i.drv_phy_test_clear)
    drv_phy_test_lock                        0x000159a9   Thumb Code    24  drv_phy_common.o(i.drv_phy_test_lock)
    drv_phy_test_write_1_byte                0x000159c1   Thumb Code    32  drv_phy_common.o(i.drv_phy_test_write_1_byte)
    drv_phy_test_write_2_byte                0x000159e1   Thumb Code    38  drv_phy_common.o(i.drv_phy_test_write_2_byte)
    drv_phy_test_write_code                  0x00015a07   Thumb Code    30  drv_phy_common.o(i.drv_phy_test_write_code)
    drv_pwr_set_pvd_mode                     0x00015a45   Thumb Code    18  drv_pwr.o(i.drv_pwr_set_pvd_mode)
    drv_pwr_set_system_clk_src               0x00015a5d   Thumb Code    44  drv_pwr.o(i.drv_pwr_set_system_clk_src)
    drv_rxbr_clear_pkt_buffer                0x00015adb   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    drv_rxbr_clear_status0                   0x00015ae5   Thumb Code     4  drv_rxbr.o(i.drv_rxbr_clear_status0)
    drv_rxbr_enable_irq                      0x00015ae9   Thumb Code    90  drv_rxbr.o(i.drv_rxbr_enable_irq)
    drv_rxbr_frame_drop_cfg                  0x00015b45   Thumb Code    16  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    drv_rxbr_get_clk                         0x00015b59   Thumb Code    66  drv_rxbr.o(i.drv_rxbr_get_clk)
    drv_rxbr_get_col_addr                    0x00015bbd   Thumb Code     4  drv_rxbr.o(i.drv_rxbr_get_col_addr)
    drv_rxbr_get_page_addr                   0x00015bd3   Thumb Code     4  drv_rxbr.o(i.drv_rxbr_get_page_addr)
    drv_rxbr_get_pkt_buf_error_status        0x00015bd7   Thumb Code    12  drv_rxbr.o(i.drv_rxbr_get_pkt_buf_error_status)
    drv_rxbr_hline_rcv0_cfg                  0x00015c0b   Thumb Code    12  drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg)
    drv_rxbr_hline_rcv1_cfg                  0x00015c17   Thumb Code    12  drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg)
    drv_rxbr_hline_rcv_cfg                   0x00015c23   Thumb Code     8  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    drv_rxbr_register_irq0_callback          0x00015c2d   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_register_irq0_callback)
    drv_rxbr_register_irq1_callback          0x00015c39   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    drv_rxbr_set_ack_pkt_header              0x00015c45   Thumb Code    20  drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header)
    drv_rxbr_set_color_format                0x00015c59   Thumb Code    20  drv_rxbr.o(i.drv_rxbr_set_color_format)
    drv_rxbr_set_filter_regs                 0x00015c6d   Thumb Code    18  drv_rxbr.o(i.drv_rxbr_set_filter_regs)
    drv_rxbr_set_inten                       0x00015c7f   Thumb Code    20  drv_rxbr.o(i.drv_rxbr_set_inten)
    drv_rxbr_set_ltpo_drop_th                0x00015c93   Thumb Code    16  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    drv_rxbr_set_usr_cfg                     0x00015ca3   Thumb Code    38  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    drv_rxbr_set_usr_col                     0x00015cc9   Thumb Code     8  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    drv_rxbr_set_usr_row                     0x00015cd1   Thumb Code     8  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    drv_swire_set_int                        0x00015cd9   Thumb Code    76  drv_swire.o(i.drv_swire_set_int)
    drv_sys_cfg_clear_all_int                0x00015d2d   Thumb Code     8  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    drv_sys_cfg_clear_pending                0x00015d39   Thumb Code    32  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    drv_sys_cfg_sel_ap_rst_lvl_trig          0x00015d61   Thumb Code    18  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_lvl_trig)
    drv_sys_cfg_set_int                      0x00015d79   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    drv_timer_enable                         0x00015db7   Thumb Code    32  drv_timer.o(i.drv_timer_enable)
    drv_timer_get_instance                   0x00015dd9   Thumb Code    10  drv_timer.o(i.drv_timer_get_instance)
    drv_timer_set_compare_val                0x00015e2d   Thumb Code    16  drv_timer.o(i.drv_timer_set_compare_val)
    drv_timer_set_int                        0x00015e3d   Thumb Code    80  drv_timer.o(i.drv_timer_set_int)
    drv_tx_phy_test_enter                    0x00015e9b   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    drv_tx_phy_test_exit                     0x00015eb7   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    drv_vidc_clear_irq                       0x00015f09   Thumb Code     8  drv_vidc.o(i.drv_vidc_clear_irq)
    drv_vidc_enable                          0x00015f11   Thumb Code    24  drv_vidc.o(i.drv_vidc_enable)
    drv_vidc_enable_irq                      0x00015f29   Thumb Code    58  drv_vidc.o(i.drv_vidc_enable_irq)
    drv_vidc_get_irq_status                  0x00015f69   Thumb Code    18  drv_vidc.o(i.drv_vidc_get_irq_status)
    drv_vidc_init_module_enable              0x00015f7d   Thumb Code    36  drv_vidc.o(i.drv_vidc_init_module_enable)
    drv_vidc_register_callback               0x00015fa5   Thumb Code     6  drv_vidc.o(i.drv_vidc_register_callback)
    drv_vidc_reset                           0x00015fb1   Thumb Code     6  drv_vidc.o(i.drv_vidc_reset)
    drv_vidc_set_dst_parameter               0x00015fb7   Thumb Code    60  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    drv_vidc_set_irqen                       0x00015ff3   Thumb Code    20  drv_vidc.o(i.drv_vidc_set_irqen)
    drv_vidc_set_mirror                      0x00016007   Thumb Code    16  drv_vidc.o(i.drv_vidc_set_mirror)
    drv_vidc_set_p2r_hcoef0                  0x00016017   Thumb Code     8  drv_vidc.o(i.drv_vidc_set_p2r_hcoef0)
    drv_vidc_set_p2r_hinitb                  0x0001601f   Thumb Code    38  drv_vidc.o(i.drv_vidc_set_p2r_hinitb)
    drv_vidc_set_p2r_hinitr                  0x00016045   Thumb Code    38  drv_vidc.o(i.drv_vidc_set_p2r_hinitr)
    drv_vidc_set_pentile_swap                0x0001606d   Thumb Code    18  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    drv_vidc_set_pu_ctrl                     0x00016085   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    drv_vidc_set_rotation                    0x0001608f   Thumb Code    16  drv_vidc.o(i.drv_vidc_set_rotation)
    drv_vidc_set_scld_hcoef0                 0x0001609f   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    drv_vidc_set_scld_hcoef1                 0x000160a9   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    drv_vidc_set_scld_step                   0x000160b3   Thumb Code    18  drv_vidc.o(i.drv_vidc_set_scld_step)
    drv_vidc_set_scld_vcoef0                 0x000160c5   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    drv_vidc_set_scld_vcoef1                 0x000160cf   Thumb Code    10  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    drv_vidc_set_src_parameter               0x000160d9   Thumb Code    22  drv_vidc.o(i.drv_vidc_set_src_parameter)
    drv_wdg_clear_counter                    0x000160f1   Thumb Code    12  drv_wdg.o(i.drv_wdg_clear_counter)
    drv_wdg_set_int                          0x00016121   Thumb Code    60  drv_wdg.o(i.drv_wdg_set_int)
    fls_clr_interrupt_flag                   0x00016161   Thumb Code    10  drv_fls.o(i.fls_clr_interrupt_flag)
    fputc                                    0x0001616b   Thumb Code    20  tau_log.o(i.fputc)
    hal_dsi_rx_ctrl_create_handle            0x000161d1   Thumb Code    48  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    hal_dsi_rx_ctrl_dsc_async_handler        0x00016205   Thumb Code    34  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dsc_async_handler)
    hal_dsi_rx_ctrl_gen_a_tear_signal        0x0001622d   Thumb Code    32  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_gen_a_tear_signal)
    hal_dsi_rx_ctrl_get_max_ret_size         0x00016255   Thumb Code    30  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size)
    hal_dsi_rx_ctrl_init                     0x0001627d   Thumb Code   144  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    hal_dsi_rx_ctrl_pre_init_pps             0x00016a6d   Thumb Code    56  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    hal_dsi_rx_ctrl_restart                  0x00016aa9   Thumb Code    72  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart)
    hal_dsi_rx_ctrl_send_ack_cmd             0x00016af9   Thumb Code   212  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd)
    hal_dsi_rx_ctrl_set_cus_esc_clk          0x00016be9   Thumb Code    34  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk)
    hal_dsi_rx_ctrl_set_cus_scld_filter      0x00016c15   Thumb Code    98  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_scld_filter)
    hal_dsi_rx_ctrl_set_cus_sync_line        0x00016c81   Thumb Code    44  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_sync_line)
    hal_dsi_rx_ctrl_set_tear_mode_ex         0x00016d5f   Thumb Code    14  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_tear_mode_ex)
    hal_dsi_rx_ctrl_start                    0x00016d6d   Thumb Code    46  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    hal_dsi_rx_ctrl_toggle_resolution        0x00016da9   Thumb Code    28  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    hal_dsi_tx_ctrl_create_handle            0x000173b5   Thumb Code    34  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    hal_dsi_tx_ctrl_enter_init_panel_mode    0x000173e1   Thumb Code    68  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_enter_init_panel_mode)
    hal_dsi_tx_ctrl_exit_init_panel_mode     0x0001742d   Thumb Code    32  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_exit_init_panel_mode)
    hal_dsi_tx_ctrl_init                     0x00017455   Thumb Code   154  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    hal_dsi_tx_ctrl_panel_reset_pin          0x0001751d   Thumb Code    12  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_panel_reset_pin)
    hal_dsi_tx_ctrl_set_ccm                  0x00017529   Thumb Code    28  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm)
    hal_dsi_tx_ctrl_set_overwrite_rgb        0x00017549   Thumb Code    16  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    hal_dsi_tx_ctrl_set_partial_disp         0x0001755d   Thumb Code    12  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp)
    hal_dsi_tx_ctrl_set_partial_disp_area    0x0001756d   Thumb Code    30  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_partial_disp_area)
    hal_dsi_tx_ctrl_start                    0x00017591   Thumb Code   150  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    hal_dsi_tx_ctrl_write_array_cmd          0x00017639   Thumb Code   236  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd)
    hal_dsi_tx_ctrl_write_cmd                0x00017729   Thumb Code   200  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    hal_gpio_get_input_data                  0x000179d9   Thumb Code    18  hal_gpio.o(i.hal_gpio_get_input_data)
    hal_gpio_init_input                      0x000179ed   Thumb Code    28  hal_gpio.o(i.hal_gpio_init_input)
    hal_gpio_init_output                     0x00017a0d   Thumb Code    34  hal_gpio.o(i.hal_gpio_init_output)
    hal_gpio_set_mode                        0x00017a35   Thumb Code    90  hal_gpio.o(i.hal_gpio_set_mode)
    hal_gpio_set_output_data                 0x00017a95   Thumb Code     8  hal_gpio.o(i.hal_gpio_set_output_data)
    hal_gpio_set_pull_state                  0x00017a9d   Thumb Code    26  hal_gpio.o(i.hal_gpio_set_pull_state)
    hal_internal_check_video_auto_sync       0x00017abd   Thumb Code    18  hal_internal_vsync.o(i.hal_internal_check_video_auto_sync)
    hal_internal_init_memc                   0x00017ad5   Thumb Code   170  hal_internal_vsync.o(i.hal_internal_init_memc)
    hal_internal_rx_dcs_async_handler        0x00017bd1   Thumb Code    42  hal_internal_vsync.o(i.hal_internal_rx_dcs_async_handler)
    hal_internal_rx_dcs_polling              0x00017bfd   Thumb Code    78  hal_internal_vsync.o(i.hal_internal_rx_dcs_polling)
    hal_internal_sync_get_fb_setting         0x00017c55   Thumb Code    12  hal_internal_vsync.o(i.hal_internal_sync_get_fb_setting)
    hal_internal_sync_get_hight_performan_mode 0x00017c65   Thumb Code    10  hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode)
    hal_internal_sync_input_resolution_change 0x00017c75   Thumb Code   438  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    hal_internal_vsync_deinit                0x00017ea1   Thumb Code    30  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    hal_internal_vsync_get_sync_line         0x00017ec9   Thumb Code    18  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    hal_internal_vsync_get_tear_mode         0x00017ee1   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_tear_mode)
    hal_internal_vsync_get_tx_state          0x00017eed   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    hal_internal_vsync_init_rx               0x00017ef9   Thumb Code   274  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    hal_internal_vsync_init_tx               0x00018039   Thumb Code   172  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    hal_internal_vsync_set_auto_hw_filter    0x000180e9   Thumb Code   132  hal_internal_vsync.o(i.hal_internal_vsync_set_auto_hw_filter)
    hal_internal_vsync_set_rx_state          0x00018179   Thumb Code    30  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    hal_internal_vsync_set_sync_line         0x0001819d   Thumb Code    64  hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line)
    hal_internal_vsync_set_tear_mode         0x000181e1   Thumb Code    72  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    hal_internal_vsync_set_tx_state          0x00018231   Thumb Code   122  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    hal_intl_svs_deinit_tx                   0x000182b5   Thumb Code    10  hal_internal_soft_sync.o(i.hal_intl_svs_deinit_tx)
    hal_intl_svs_handle                      0x000182c5   Thumb Code    24  hal_internal_soft_sync.o(i.hal_intl_svs_handle)
    hal_intl_svs_init_rx                     0x000182e9   Thumb Code   108  hal_internal_soft_sync.o(i.hal_intl_svs_init_rx)
    hal_intl_svs_init_tx                     0x00018361   Thumb Code    16  hal_internal_soft_sync.o(i.hal_intl_svs_init_tx)
    hal_intl_svs_set_sync_coef               0x00018375   Thumb Code     8  hal_internal_soft_sync.o(i.hal_intl_svs_set_sync_coef)
    hal_intl_svs_update_rxbr_clk             0x00018381   Thumb Code    52  hal_internal_soft_sync.o(i.hal_intl_svs_update_rxbr_clk)
    hal_system_enable_systick                0x00018829   Thumb Code     8  hal_system.o(i.hal_system_enable_systick)
    hal_system_get_tick                      0x00018831   Thumb Code     8  hal_system.o(i.hal_system_get_tick)
    hal_system_init                          0x00018839   Thumb Code   104  hal_system.o(i.hal_system_init)
    hal_system_init_console                  0x000188c1   Thumb Code    28  hal_system.o(i.hal_system_init_console)
    hal_system_set_phy_calibration           0x000188dd   Thumb Code     8  hal_system.o(i.hal_system_set_phy_calibration)
    hal_uart_init                            0x00018915   Thumb Code   126  hal_uart.o(i.hal_uart_init)
    hal_uart_transmit_blocking               0x000189a1   Thumb Code    12  hal_uart.o(i.hal_uart_transmit_blocking)
    handle_init                              0x000189b1   Thumb Code   140  irq_redirect .o(i.handle_init)
    main                                     0x00018bcd   Thumb Code    10  main.o(i.main)
    sqrt                                     0x00019949   Thumb Code    66  sqrt.o(i.sqrt)
    panel_init_code                          0x0001a0ec   Data        7814  ap_demo.o(.constdata)
    Region$$Table$$Base                      0x0001c45c   Number         0  anon$$obj.o(Region$$Table)
    Region$$Table$$Limit                     0x0001c48c   Number         0  anon$$obj.o(Region$$Table)
    g_fun_handle                             0x00070100   Data         192  irq_redirect .o(.ARM.__AT_0x00070100)
    s_power_up_flag                          0x000701d7   Data           1  ap_demo.o(.data)
    panel_mode                               0x000701d8   Data           1  ap_demo.o(.data)
    s_tp_delay_count                         0x000701e6   Data           2  ap_demo.o(.data)
    panel_r                                  0x000701e8   Data           2  ap_demo.o(.data)
    panel_g                                  0x000701ea   Data           2  ap_demo.o(.data)
    panel_b                                  0x000701ec   Data           2  ap_demo.o(.data)
    s_heartbeat                              0x000701fc   Data           4  ap_demo.o(.data)
    rx_filter_1080_h_4_96                    0x00070208   Data         256  ap_demo.o(.data)
    rx_filter_2400_v_4_96                    0x00070308   Data         256  ap_demo.o(.data)
    g_tp_sleep_delay_count                   0x00070408   Data           1  app_tp_st_touch.o(.data)
    g_tp_wakeup_response                     0x00070409   Data           1  app_tp_st_touch.o(.data)
    s_tp_wakeup                              0x0007040a   Data           1  app_tp_st_touch.o(.data)
    st_touch_init_sensor_off                 0x0007040d   Data           3  app_tp_st_touch.o(.data)
    st_touch_init_sensor_on                  0x00070410   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_reset                 0x00070413   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_FpnlInit              0x00070416   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_PnlInit               0x00070419   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_SvCfg                 0x0007041c   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_SvCx                  0x0007041f   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_SvPnl                 0x00070422   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_clearfifo             0x00070425   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_clkreset              0x00070428   Data           3  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_TuneM                 0x0007042b   Data           4  app_tp_st_touch.o(.data)
    st_touch_tp_tuning_TuneS                 0x0007042f   Data           4  app_tp_st_touch.o(.data)
    phone_reg_coord_back_X61                 0x00070433   Data          16  app_tp_st_touch.o(.data)
    phone_data_E4                            0x00070444   Data           1  app_tp_for_custom_s8.o(.data)
    tp_flag                                  0x00070445   Data           1  app_tp_for_custom_s8.o(.data)
    g_phone_output_int_pad                   0x00070446   Data           1  app_tp_for_custom_s8.o(.data)
    tp_sleep_in                              0x00070447   Data           1  app_tp_for_custom_s8.o(.data)
    tp_sleep_count                           0x00070448   Data           1  app_tp_for_custom_s8.o(.data)
    sleep_double_EN                          0x00070449   Data           1  app_tp_for_custom_s8.o(.data)
    Flag_EA_EN                               0x0007044a   Data           1  app_tp_for_custom_s8.o(.data)
    Flag_touch_count                         0x0007044b   Data           1  app_tp_for_custom_s8.o(.data)
    touchnum_bak                             0x0007044c   Data           1  app_tp_for_custom_s8.o(.data)
    Flag_blacklight_EN                       0x0007044d   Data           1  app_tp_for_custom_s8.o(.data)
    phone_data_B1                            0x00070456   Data           2  app_tp_for_custom_s8.o(.data)
    phone_reg_coord_back                     0x00070460   Data         200  app_tp_for_custom_s8.o(.data)
    g_sof_gen_te_func                        0x0007053c   Data           4  hal_internal_vsync.o(.data)
    g_systick_cb_func                        0x00070550   Data           4  drv_common.o(.data)
    g_system_clock                           0x00070554   Data           4  drv_common.o(.data)
    g_scld_fhd_filter_h                      0x00070564   Data         256  drv_param_init.o(.data)
    g_scld_fhd_filter_v                      0x00070664   Data         256  drv_param_init.o(.data)
    g_scld_hd_filter_h                       0x00070764   Data         256  drv_param_init.o(.data)
    g_scld_hd_filter_v                       0x00070864   Data         256  drv_param_init.o(.data)
    g_sclu_lanczos_filter                    0x00070964   Data         128  drv_param_init.o(.data)
    g_ccm_setting                            0x000709e4   Data          36  drv_param_init.o(.data)
    g_int_rxbr_irq0_cb_func                  0x00070a10   Data           4  drv_rxbr.o(.data)
    g_int_rxbr_irq1_cb_func                  0x00070a14   Data           4  drv_rxbr.o(.data)
    g_int_vidc_cb_func                       0x00070a18   Data           4  drv_vidc.o(.data)
    g_fls_w_cmd                              0x00070a2c   Data           1  norflash.o(.data)
    g_fls_r_cmd                              0x00070a2d   Data           1  norflash.o(.data)
    g_fls_write_en_status                    0x00070a2e   Data           1  norflash.o(.data)
    isFlsTransferEnd                         0x00070a2f   Data           1  norflash.o(.data)
    isFlsFifoReq                             0x00070a30   Data           1  norflash.o(.data)
    isNandWriteCompleted                     0x00070a31   Data           1  norflash.o(.data)
    isNandReadCompleted                      0x00070a32   Data           1  norflash.o(.data)
    g_fls_error_info                         0x00070a38   Data           6  norflash.o(.data)
    __stdout                                 0x00070ab8   Data           4  stdout.o(.data)
    string                                   0x00070bf4   Data         256  tau_log.o(.bss)
    hal_dmahandle                            0x00070cf4   Data         160  hal_uart.o(.bss)
    hal_uarthandle_dma                       0x00070d94   Data          32  hal_uart.o(.bss)
    hal_uart_handle_global                   0x00070db4   Data          16  hal_uart.o(.bss)
    g_vsync_hande                            0x00070dc4   Data          84  hal_internal_vsync.o(.bss)
    g_dcs_execute_table                      0x00070e18   Data        2048  hal_internal_vsync.o(.bss)
    g_spis_ctrl_handle                       0x000717d4   Data          32  hal_spi_slave.o(.bss)
    g_packet_fifo                            0x000717f4   Data        4144  dcs_packet_fifo.o(.bss)
    __stack_limit                            0x00072828   Data           0  startup_armcm0.o(STACK)
    __initial_sp                             0x00073828   Data           0  startup_armcm0.o(STACK)



==============================================================================

Memory Map of the image

  Image Entry point : 0x000100c1

  Load Region LR_IROM2 (Base: 0x00010000, Size: 0x0000cd7c, Max: 0x00010000, ABSOLUTE, COMPRESSED[0x0000c9b8])

    Execution Region ER_IROM2 (Exec base: 0x00010000, Load base: 0x00010000, Size: 0x0000c48c, Max: 0x00010000, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00010000   0x00010000   0x000000c0   Data   RO          567    RESET               startup_armcm0.o
    0x000100c0   0x000100c0   0x00000000   Code   RO         2745  * .ARM.Collect$$$$00000000  mc_p.l(entry.o)
    0x000100c0   0x000100c0   0x00000004   Code   RO         3057    .ARM.Collect$$$$00000001  mc_p.l(entry2.o)
    0x000100c4   0x000100c4   0x00000004   Code   RO         3060    .ARM.Collect$$$$00000004  mc_p.l(entry5.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         3062    .ARM.Collect$$$$00000008  mc_p.l(entry7b.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         3064    .ARM.Collect$$$$0000000A  mc_p.l(entry8b.o)
    0x000100c8   0x000100c8   0x00000008   Code   RO         3065    .ARM.Collect$$$$0000000B  mc_p.l(entry9a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         3067    .ARM.Collect$$$$0000000D  mc_p.l(entry10a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         3069    .ARM.Collect$$$$0000000F  mc_p.l(entry11a.o)
    0x000100d0   0x000100d0   0x00000004   Code   RO         3058    .ARM.Collect$$$$00002712  mc_p.l(entry2.o)
    0x000100d4   0x000100d4   0x00000078   Code   RO          568    .text               startup_armcm0.o
    0x0001014c   0x0001014c   0x0000002c   Code   RO         2748    .text               mc_p.l(uidiv.o)
    0x00010178   0x00010178   0x00000028   Code   RO         2750    .text               mc_p.l(idiv.o)
    0x000101a0   0x000101a0   0x00000024   Code   RO         2752    .text               mc_p.l(memcpya.o)
    0x000101c4   0x000101c4   0x00000024   Code   RO         2754    .text               mc_p.l(memseta.o)
    0x000101e8   0x000101e8   0x000000b2   Code   RO         3019    .text               mf_p.l(fadd.o)
    0x0001029a   0x0001029a   0x0000007a   Code   RO         3021    .text               mf_p.l(fmul.o)
    0x00010314   0x00010314   0x0000007c   Code   RO         3023    .text               mf_p.l(fdiv.o)
    0x00010390   0x00010390   0x00000018   Code   RO         3025    .text               mf_p.l(fscalb.o)
    0x000103a8   0x000103a8   0x00000164   Code   RO         3027    .text               mf_p.l(dadd.o)
    0x0001050c   0x0001050c   0x000000d0   Code   RO         3029    .text               mf_p.l(dmul.o)
    0x000105dc   0x000105dc   0x000000f0   Code   RO         3031    .text               mf_p.l(ddiv.o)
    0x000106cc   0x000106cc   0x00000016   Code   RO         3033    .text               mf_p.l(fflti.o)
    0x000106e2   0x000106e2   0x0000000e   Code   RO         3035    .text               mf_p.l(ffltui.o)
    0x000106f0   0x000106f0   0x0000001c   Code   RO         3039    .text               mf_p.l(dfltui.o)
    0x0001070c   0x0001070c   0x00000032   Code   RO         3041    .text               mf_p.l(ffixi.o)
    0x0001073e   0x0001073e   0x00000028   Code   RO         3043    .text               mf_p.l(ffixui.o)
    0x00010766   0x00010766   0x00000002   PAD
    0x00010768   0x00010768   0x00000048   Code   RO         3045    .text               mf_p.l(dfixi.o)
    0x000107b0   0x000107b0   0x0000003c   Code   RO         3047    .text               mf_p.l(dfixui.o)
    0x000107ec   0x000107ec   0x00000028   Code   RO         3049    .text               mf_p.l(f2d.o)
    0x00010814   0x00010814   0x00000028   Code   RO         3051    .text               mf_p.l(cdcmple.o)
    0x0001083c   0x0001083c   0x00000014   Code   RO         3053    .text               mf_p.l(cfcmple.o)
    0x00010850   0x00010850   0x00000014   Code   RO         3055    .text               mf_p.l(cfrcmple.o)
    0x00010864   0x00010864   0x00000060   Code   RO         3072    .text               mc_p.l(uldiv.o)
    0x000108c4   0x000108c4   0x00000020   Code   RO         3074    .text               mc_p.l(llshl.o)
    0x000108e4   0x000108e4   0x00000022   Code   RO         3076    .text               mc_p.l(llushr.o)
    0x00010906   0x00010906   0x00000026   Code   RO         3078    .text               mc_p.l(llsshr.o)
    0x0001092c   0x0001092c   0x00000000   Code   RO         3087    .text               mc_p.l(iusefp.o)
    0x0001092c   0x0001092c   0x00000082   Code   RO         3088    .text               mf_p.l(fepilogue.o)
    0x000109ae   0x000109ae   0x000000be   Code   RO         3090    .text               mf_p.l(depilogue.o)
    0x00010a6c   0x00010a6c   0x000000a2   Code   RO         3094    .text               mf_p.l(dsqrt.o)
    0x00010b0e   0x00010b0e   0x00000002   PAD
    0x00010b10   0x00010b10   0x00000040   Code   RO         3096    .text               mf_p.l(dfixul.o)
    0x00010b50   0x00010b50   0x00000028   Code   RO         3098    .text               mf_p.l(cdrcmple.o)
    0x00010b78   0x00010b78   0x00000024   Code   RO         3100    .text               mc_p.l(init.o)
    0x00010b9c   0x00010b9c   0x00000056   Code   RO         3110    .text               mc_p.l(__dczerorl2.o)
    0x00010bf2   0x00010bf2   0x00000002   PAD
    0x00010bf4   0x00010bf4   0x00000018   Code   RO         2189    i.ADC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c0c   0x00010c0c   0x00000018   Code   RO         2190    i.AP_NRESET_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c24   0x00010c24   0x00000014   Code   RO         2191    i.DMA_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c38   0x00010c38   0x0000001c   Code   RO         2192    i.EXTI_INT0_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c54   0x00010c54   0x0000001c   Code   RO         2193    i.EXTI_INT1_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c70   0x00010c70   0x0000001c   Code   RO         2194    i.EXTI_INT2_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010c8c   0x00010c8c   0x0000001c   Code   RO         2195    i.EXTI_INT3_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010ca8   0x00010ca8   0x0000001c   Code   RO         2196    i.EXTI_INT4_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010cc4   0x00010cc4   0x0000001c   Code   RO         2197    i.EXTI_INT5_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010ce0   0x00010ce0   0x0000001c   Code   RO         2198    i.EXTI_INT6_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010cfc   0x00010cfc   0x0000001c   Code   RO         2199    i.EXTI_INT7_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010d18   0x00010d18   0x00000014   Code   RO         2200    i.FLSCTRL_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010d2c   0x00010d2c   0x0000004e   Code   RO          103    i.Gpio_swire_output  ap_demo.o
    0x00010d7a   0x00010d7a   0x00000002   PAD
    0x00010d7c   0x00010d7c   0x00000014   Code   RO         2201    i.HardFault_Handler  CVWL568.lib(irq_redirect .o)
    0x00010d90   0x00010d90   0x00000018   Code   RO         2202    i.I2C0_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010da8   0x00010da8   0x00000018   Code   RO         2203    i.I2C1_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010dc0   0x00010dc0   0x00000018   Code   RO         2204    i.LCDC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010dd8   0x00010dd8   0x00000028   Code   RO         1074    i.LOG_printf        CVWL568.lib(tau_log.o)
    0x00010e00   0x00010e00   0x00000018   Code   RO         2205    i.MEMC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e18   0x00010e18   0x00000018   Code   RO         2206    i.MIPI_RX_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e30   0x00010e30   0x00000018   Code   RO         2207    i.MIPI_TX_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e48   0x00010e48   0x0000001c   Code   RO         2208    i.PWMDET_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010e64   0x00010e64   0x000000c4   Code   RO          104    i.PhoneDisOffDeal   ap_demo.o
    0x00010f28   0x00010f28   0x0000001c   Code   RO         2209    i.SPIM_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010f44   0x00010f44   0x0000001c   Code   RO         2210    i.SPIS_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010f60   0x00010f60   0x0000001c   Code   RO         2211    i.SWIRE_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010f7c   0x00010f7c   0x00000018   Code   RO         2212    i.SysTick_Handler   CVWL568.lib(irq_redirect .o)
    0x00010f94   0x00010f94   0x00000018   Code   RO         2213    i.TIMER0_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010fac   0x00010fac   0x00000018   Code   RO         2214    i.TIMER1_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010fc4   0x00010fc4   0x00000018   Code   RO         2215    i.TIMER2_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010fdc   0x00010fdc   0x00000018   Code   RO         2216    i.TIMER3_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00010ff4   0x00010ff4   0x00000002   Code   RO         2616    i.UART_DisableDma   CVWL568.lib(drv_uart.o)
    0x00010ff6   0x00010ff6   0x00000004   Code   RO         2622    i.UART_GetInstance  CVWL568.lib(drv_uart.o)
    0x00010ffa   0x00010ffa   0x00000002   Code   RO         3105    i.__scatterload_null  mc_p.l(handlers.o)
    0x00010ffc   0x00010ffc   0x00000004   Code   RO         1766    i.drv_dsi_rx_set_inten  CVWL568.lib(drv_dsi_rx.o)
    0x00011000   0x00011000   0x00000014   Data   RO         1211    .ARM.__at_0x11000   CVWL568.lib(drv_common.o)
    0x00011014   0x00011014   0x00000004   Code   RO         1813    i.drv_dsi_tx_command_put_payload  CVWL568.lib(drv_dsi_tx.o)
    0x00011018   0x00011018   0x00000004   Data   RO         1212    .ARM.__at_0x11018   CVWL568.lib(drv_common.o)
    0x0001101c   0x0001101c   0x0000001c   Code   RO         2612    i.UART0_IRQ_Handle  CVWL568.lib(drv_uart.o)
    0x00011038   0x00011038   0x00000018   Code   RO         2217    i.UART_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00011050   0x00011050   0x00000024   Code   RO         2630    i.UART_ResetRxFIFO  CVWL568.lib(drv_uart.o)
    0x00011074   0x00011074   0x00000048   Code   RO         2633    i.UART_SetBaudRate  CVWL568.lib(drv_uart.o)
    0x000110bc   0x000110bc   0x0000001a   Code   RO         2634    i.UART_SwitchSCLK   CVWL568.lib(drv_uart.o)
    0x000110d6   0x000110d6   0x00000134   Code   RO         2636    i.UART_TransferHandleIRQ  CVWL568.lib(drv_uart.o)
    0x0001120a   0x0001120a   0x0000001a   Code   RO         2638    i.UART_WriteBlocking  CVWL568.lib(drv_uart.o)
    0x00011224   0x00011224   0x000000bc   Code   RO         2639    i.UART_init         CVWL568.lib(drv_uart.o)
    0x000112e0   0x000112e0   0x00000018   Code   RO         2218    i.VIDC_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x000112f8   0x000112f8   0x00000018   Code   RO         2219    i.VPRE_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00011310   0x00011310   0x00000018   Code   RO         2220    i.WDG_IRQn_Handler  CVWL568.lib(irq_redirect .o)
    0x00011328   0x00011328   0x00000020   Code   RO         2991    i.__0printf         mc_p.l(printfa.o)
    0x00011348   0x00011348   0x00000024   Code   RO         2997    i.__0vsprintf       mc_p.l(printfa.o)
    0x0001136c   0x0001136c   0x0000002e   Code   RO         3092    i.__ARM_clz         mf_p.l(depilogue.o)
    0x0001139a   0x0001139a   0x0000001a   Code   RO          797    i.__ARM_common_switch8  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000113b4   0x000113b4   0x00000018   Code   RO         1656    i.__NVIC_ClearPendingIRQ  CVWL568.lib(drv_spi_master.o)
    0x000113cc   0x000113cc   0x00000020   Code   RO         2037    i.__NVIC_DisableIRQ  CVWL568.lib(drv_rxbr.o)
    0x000113ec   0x000113ec   0x00000018   Code   RO         2038    i.__NVIC_EnableIRQ  CVWL568.lib(drv_rxbr.o)
    0x00011404   0x00011404   0x00000044   Code   RO         2339    i.__NVIC_SetPriority  CVWL568.lib(hal_spi_slave.o)
    0x00011448   0x00011448   0x0000000e   Code   RO         3104    i.__scatterload_copy  mc_p.l(handlers.o)
    0x00011456   0x00011456   0x0000000e   Code   RO         3106    i.__scatterload_zeroinit  mc_p.l(handlers.o)
    0x00011464   0x00011464   0x0000000c   Code   RO         3082    i.__set_errno       mc_p.l(errno.o)
    0x00011470   0x00011470   0x00000174   Code   RO         2998    i._fp_digits        mc_p.l(printfa.o)
    0x000115e4   0x000115e4   0x000006ec   Code   RO         2999    i._printf_core      mc_p.l(printfa.o)
    0x00011cd0   0x00011cd0   0x00000020   Code   RO         3000    i._printf_post_padding  mc_p.l(printfa.o)
    0x00011cf0   0x00011cf0   0x0000002c   Code   RO         3001    i._printf_pre_padding  mc_p.l(printfa.o)
    0x00011d1c   0x00011d1c   0x0000000a   Code   RO         3003    i._sputc            mc_p.l(printfa.o)
    0x00011d26   0x00011d26   0x00000002   PAD
    0x00011d28   0x00011d28   0x00001078   Code   RO          105    i.ap_dcs_read       ap_demo.o
    0x00012da0   0x00012da0   0x00000124   Code   RO          106    i.ap_demo           ap_demo.o
    0x00012ec4   0x00012ec4   0x0000004c   Code   RO          107    i.ap_get_reg_df     ap_demo.o
    0x00012f10   0x00012f10   0x00000020   Code   RO          423    i.ap_get_tp_calibration_status_01  app_tp_st_touch.o
    0x00012f30   0x00012f30   0x00000074   Code   RO          108    i.ap_set_backlight_51  ap_demo.o
    0x00012fa4   0x00012fa4   0x00000044   Code   RO          109    i.ap_set_display_off  ap_demo.o
    0x00012fe8   0x00012fe8   0x00000038   Code   RO          110    i.ap_set_display_on  ap_demo.o
    0x00013020   0x00013020   0x00000080   Code   RO          111    i.ap_set_enter_sleep_mode  ap_demo.o
    0x000130a0   0x000130a0   0x00000070   Code   RO          112    i.ap_set_exit_sleep_mode  ap_demo.o
    0x00013110   0x00013110   0x00000030   Code   RO          113    i.ap_set_hbm_53     ap_demo.o
    0x00013140   0x00013140   0x00000028   Code   RO          114    i.ap_update_frame_rate  ap_demo.o
    0x00013168   0x00013168   0x0000001c   Code   RO         2039    i.app_ADC_IRQn_Handler  CVWL568.lib(drv_rxbr.o)
    0x00013184   0x00013184   0x00000024   Code   RO         1456    i.app_AP_NRESET_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x000131a8   0x000131a8   0x0000001c   Code   RO         1457    i.app_EXTI_INT0_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x000131c4   0x000131c4   0x0000001c   Code   RO         1458    i.app_EXTI_INT1_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x000131e0   0x000131e0   0x0000001c   Code   RO         1459    i.app_EXTI_INT2_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x000131fc   0x000131fc   0x0000001c   Code   RO         1460    i.app_EXTI_INT3_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00013218   0x00013218   0x0000001c   Code   RO         1461    i.app_EXTI_INT4_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00013234   0x00013234   0x0000001c   Code   RO         1462    i.app_EXTI_INT5_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00013250   0x00013250   0x0000001c   Code   RO         1463    i.app_EXTI_INT6_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x0001326c   0x0001326c   0x0000001c   Code   RO         1464    i.app_EXTI_INT7_IRQn_Handler  CVWL568.lib(drv_gpio.o)
    0x00013288   0x00013288   0x00000048   Code   RO         1203    i.app_HardFault_Handler  CVWL568.lib(drv_common.o)
    0x000132d0   0x000132d0   0x00000018   Code   RO         1567    i.app_I2C0_IRQn_Handler  CVWL568.lib(drv_i2c_slave.o)
    0x000132e8   0x000132e8   0x00000010   Code   RO         1533    i.app_I2C1_IRQn_Handler  CVWL568.lib(drv_i2c_master.o)
    0x000132f8   0x000132f8   0x00000130   Code   RO         1104    i.app_LCDC_IRQn_Handler  CVWL568.lib(hal_internal_vsync.o)
    0x00013428   0x00013428   0x00000088   Code   RO         1981    i.app_MEMC_IRQn_Handler  CVWL568.lib(drv_memc.o)
    0x000134b0   0x000134b0   0x00000298   Code   RO         1751    i.app_MIPI_RX_IRQn_Handler  CVWL568.lib(drv_dsi_rx.o)
    0x00013748   0x00013748   0x000000a0   Code   RO         1809    i.app_MIPI_TX_IRQn_Handler  CVWL568.lib(drv_dsi_tx.o)
    0x000137e8   0x000137e8   0x00000048   Code   RO         2493    i.app_PWMDET_IRQn_Handler  CVWL568.lib(drv_pwm.o)
    0x00013830   0x00013830   0x00000030   Code   RO         1657    i.app_SPIM_IRQn_Handler  CVWL568.lib(drv_spi_master.o)
    0x00013860   0x00013860   0x00000200   Code   RO         2340    i.app_SPIS_IRQn_Handler  CVWL568.lib(hal_spi_slave.o)
    0x00013a60   0x00013a60   0x00000020   Code   RO         2558    i.app_SWIRE_IRQn_Handler  CVWL568.lib(drv_swire.o)
    0x00013a80   0x00013a80   0x00000018   Code   RO         1204    i.app_SysTick_Handler  CVWL568.lib(drv_common.o)
    0x00013a98   0x00013a98   0x0000000a   Code   RO         2577    i.app_TIMER0_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x00013aa2   0x00013aa2   0x0000000a   Code   RO         2578    i.app_TIMER1_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x00013aac   0x00013aac   0x0000000a   Code   RO         2579    i.app_TIMER2_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x00013ab6   0x00013ab6   0x0000000a   Code   RO         2580    i.app_TIMER3_IRQn_Handler  CVWL568.lib(drv_timer.o)
    0x00013ac0   0x00013ac0   0x00000008   Code   RO         2640    i.app_UART_IRQn_Handler  CVWL568.lib(drv_uart.o)
    0x00013ac8   0x00013ac8   0x0000001c   Code   RO         2110    i.app_VIDC_IRQn_Handler  CVWL568.lib(drv_vidc.o)
    0x00013ae4   0x00013ae4   0x0000001c   Code   RO         2040    i.app_VPRE_IRQn_Handler  CVWL568.lib(drv_rxbr.o)
    0x00013b00   0x00013b00   0x00000038   Code   RO         2699    i.app_WDG_IRQn_Handler  CVWL568.lib(drv_wdg.o)
    0x00013b38   0x00013b38   0x00000010   Code   RO         1318    i.app_dma_irq_handler  CVWL568.lib(drv_dma.o)
    0x00013b48   0x00013b48   0x00000030   Code   RO         2382    i.app_fls_ctrl_Handler  CVWL568.lib(norflash.o)
    0x00013b78   0x00013b78   0x00000024   Code   RO          547    i.board_Init        board.o
    0x00013b9c   0x00013b9c   0x0000058c   Code   RO         1105    i.calc_framebuffer_setting  CVWL568.lib(hal_internal_vsync.o)
    0x00014128   0x00014128   0x000000c8   Code   RO         2734    i.ceil              m_ps.l(ceil.o)
    0x000141f0   0x000141f0   0x0000002c   Code   RO         1106    i.check_mipi_rx_tx_video_info  CVWL568.lib(hal_internal_vsync.o)
    0x0001421c   0x0001421c   0x00000084   Code   RO         1107    i.check_pkt_buf_rev  CVWL568.lib(hal_internal_vsync.o)
    0x000142a0   0x000142a0   0x00000058   Code   RO         2722    i.dcs_packet_fifo_alloc  CVWL568.lib(dcs_packet_fifo.o)
    0x000142f8   0x000142f8   0x00000018   Code   RO         2723    i.dcs_packet_fifo_init  CVWL568.lib(dcs_packet_fifo.o)
    0x00014310   0x00014310   0x00000044   Code   RO         2724    i.dcs_packet_free_fifo_header  CVWL568.lib(dcs_packet_fifo.o)
    0x00014354   0x00014354   0x00000024   Code   RO         2725    i.dcs_packet_get_fifo_header  CVWL568.lib(dcs_packet_fifo.o)
    0x00014378   0x00014378   0x0000002c   Code   RO         1108    i.dcs_sw_filter     CVWL568.lib(hal_internal_vsync.o)
    0x000143a4   0x000143a4   0x00000018   Code   RO         1066    i.delayMs           CVWL568.lib(tau_delay.o)
    0x000143bc   0x000143bc   0x00000022   Code   RO         1067    i.delayUs           CVWL568.lib(tau_delay.o)
    0x000143de   0x000143de   0x00000002   PAD
    0x000143e0   0x000143e0   0x00000038   Code   RO         1689    i.drv_ap_rst_trig_edge_detect  CVWL568.lib(drv_sys_cfg.o)
    0x00014418   0x00014418   0x0000000c   Code   RO         2310    i.drv_chip_info_get_info  CVWL568.lib(drv_chip_info.o)
    0x00014424   0x00014424   0x00000040   Code   RO         2311    i.drv_chip_info_init  CVWL568.lib(drv_chip_info.o)
    0x00014464   0x00014464   0x000000b0   Code   RO         2312    i.drv_chip_rx_info_check  CVWL568.lib(drv_chip_info.o)
    0x00014514   0x00014514   0x00000014   Code   RO         2313    i.drv_chip_rx_init_done  CVWL568.lib(drv_chip_info.o)
    0x00014528   0x00014528   0x00000058   Code   RO         1206    i.drv_common_enable_systick  CVWL568.lib(drv_common.o)
    0x00014580   0x00014580   0x0000000c   Code   RO         1207    i.drv_common_get_tick  CVWL568.lib(drv_common.o)
    0x0001458c   0x0001458c   0x00000008   Code   RO         1209    i.drv_common_system_init  CVWL568.lib(drv_common.o)
    0x00014594   0x00014594   0x00000010   Code   RO         1231    i.drv_crgu_config_reset_modules  CVWL568.lib(drv_crgu.o)
    0x000145a4   0x000145a4   0x00000014   Code   RO         1244    i.drv_crgu_set_ahb_pre_div  CVWL568.lib(drv_crgu.o)
    0x000145b8   0x000145b8   0x00000014   Code   RO         1245    i.drv_crgu_set_ahb_src  CVWL568.lib(drv_crgu.o)
    0x000145cc   0x000145cc   0x00000020   Code   RO         1248    i.drv_crgu_set_clock  CVWL568.lib(drv_crgu.o)
    0x000145ec   0x000145ec   0x00000014   Code   RO         1249    i.drv_crgu_set_dpi_mux_src  CVWL568.lib(drv_crgu.o)
    0x00014600   0x00014600   0x00000018   Code   RO         1250    i.drv_crgu_set_dpi_pre_div  CVWL568.lib(drv_crgu.o)
    0x00014618   0x00014618   0x00000014   Code   RO         1251    i.drv_crgu_set_dpi_pre_src  CVWL568.lib(drv_crgu.o)
    0x0001462c   0x0001462c   0x00000014   Code   RO         1252    i.drv_crgu_set_dsc_core_div  CVWL568.lib(drv_crgu.o)
    0x00014640   0x00014640   0x00000014   Code   RO         1253    i.drv_crgu_set_dsco_src  CVWL568.lib(drv_crgu.o)
    0x00014654   0x00014654   0x00000014   Code   RO         1254    i.drv_crgu_set_dsco_src_div  CVWL568.lib(drv_crgu.o)
    0x00014668   0x00014668   0x00000014   Code   RO         1255    i.drv_crgu_set_fb_div  CVWL568.lib(drv_crgu.o)
    0x0001467c   0x0001467c   0x00000014   Code   RO         1256    i.drv_crgu_set_fb_src  CVWL568.lib(drv_crgu.o)
    0x00014690   0x00014690   0x00000014   Code   RO         1259    i.drv_crgu_set_lcdc_div  CVWL568.lib(drv_crgu.o)
    0x000146a4   0x000146a4   0x00000014   Code   RO         1260    i.drv_crgu_set_lcdc_src  CVWL568.lib(drv_crgu.o)
    0x000146b8   0x000146b8   0x00000014   Code   RO         1261    i.drv_crgu_set_mipi_cfg_src  CVWL568.lib(drv_crgu.o)
    0x000146cc   0x000146cc   0x00000018   Code   RO         1262    i.drv_crgu_set_mipi_ref_src  CVWL568.lib(drv_crgu.o)
    0x000146e4   0x000146e4   0x00000018   Code   RO         1265    i.drv_crgu_set_reset  CVWL568.lib(drv_crgu.o)
    0x000146fc   0x000146fc   0x00000014   Code   RO         1266    i.drv_crgu_set_rxbr_div  CVWL568.lib(drv_crgu.o)
    0x00014710   0x00014710   0x00000014   Code   RO         1267    i.drv_crgu_set_rxbr_src  CVWL568.lib(drv_crgu.o)
    0x00014724   0x00014724   0x00000014   Code   RO         1269    i.drv_crgu_set_vidc_src  CVWL568.lib(drv_crgu.o)
    0x00014738   0x00014738   0x00000018   Code   RO         1322    i.drv_dma_clear_flag  CVWL568.lib(drv_dma.o)
    0x00014750   0x00014750   0x0000000c   Code   RO         1330    i.drv_dma_get_channel_flag  CVWL568.lib(drv_dma.o)
    0x0001475c   0x0001475c   0x00000090   Code   RO         1333    i.drv_dma_irq_handler  CVWL568.lib(drv_dma.o)
    0x000147ec   0x000147ec   0x00000036   Code   RO         2323    i.drv_dsc_dec_convert_pps_rc_parameter  CVWL568.lib(drv_dsc_dec.o)
    0x00014822   0x00014822   0x0000000c   Code   RO         2324    i.drv_dsc_dec_disable  CVWL568.lib(drv_dsc_dec.o)
    0x0001482e   0x0001482e   0x00000002   PAD
    0x00014830   0x00014830   0x00000074   Code   RO         2325    i.drv_dsc_dec_enable  CVWL568.lib(drv_dsc_dec.o)
    0x000148a4   0x000148a4   0x0000000a   Code   RO         2326    i.drv_dsc_dec_get_nslc  CVWL568.lib(drv_dsc_dec.o)
    0x000148ae   0x000148ae   0x00000028   Code   RO         2328    i.drv_dsc_dec_set_u8_pps  CVWL568.lib(drv_dsc_dec.o)
    0x000148d6   0x000148d6   0x00000002   PAD
    0x000148d8   0x000148d8   0x00000104   Code   RO         1752    i.drv_dsi_rx_calc_ipi_tx_delay  CVWL568.lib(drv_dsi_rx.o)
    0x000149dc   0x000149dc   0x00000040   Code   RO         1753    i.drv_dsi_rx_enable_irq  CVWL568.lib(drv_dsi_rx.o)
    0x00014a1c   0x00014a1c   0x0000000e   Code   RO         1754    i.drv_dsi_rx_get_bta_status  CVWL568.lib(drv_dsi_rx.o)
    0x00014a2a   0x00014a2a   0x00000002   PAD
    0x00014a2c   0x00014a2c   0x00000050   Code   RO         1755    i.drv_dsi_rx_get_color_bpp  CVWL568.lib(drv_dsi_rx.o)
    0x00014a7c   0x00014a7c   0x0000001c   Code   RO         1756    i.drv_dsi_rx_get_color_pcc  CVWL568.lib(drv_dsi_rx.o)
    0x00014a98   0x00014a98   0x00000008   Code   RO         1757    i.drv_dsi_rx_get_compression_en  CVWL568.lib(drv_dsi_rx.o)
    0x00014aa0   0x00014aa0   0x00000006   Code   RO         1758    i.drv_dsi_rx_get_max_ret_size  CVWL568.lib(drv_dsi_rx.o)
    0x00014aa6   0x00014aa6   0x0000000e   Code   RO         1762    i.drv_dsi_rx_power_up  CVWL568.lib(drv_dsi_rx.o)
    0x00014ab4   0x00014ab4   0x00000020   Code   RO         1763    i.drv_dsi_rx_set_ctrl_cfg  CVWL568.lib(drv_dsi_rx.o)
    0x00014ad4   0x00014ad4   0x00000010   Code   RO         1764    i.drv_dsi_rx_set_ddi_cfg  CVWL568.lib(drv_dsi_rx.o)
    0x00014ae4   0x00014ae4   0x00000010   Code   RO         1767    i.drv_dsi_rx_set_ipi_cfg  CVWL568.lib(drv_dsi_rx.o)
    0x00014af4   0x00014af4   0x00000046   Code   RO         1769    i.drv_dsi_rx_set_lane_swap  CVWL568.lib(drv_dsi_rx.o)
    0x00014b3a   0x00014b3a   0x00000026   Code   RO         1770    i.drv_dsi_rx_set_resp_cnt  CVWL568.lib(drv_dsi_rx.o)
    0x00014b60   0x00014b60   0x00000104   Code   RO         1771    i.drv_dsi_rx_set_up_phy  CVWL568.lib(drv_dsi_rx.o)
    0x00014c64   0x00014c64   0x0000000e   Code   RO         1772    i.drv_dsi_rx_shut_down  CVWL568.lib(drv_dsi_rx.o)
    0x00014c72   0x00014c72   0x00000014   Code   RO         1811    i.drv_dsi_tx_command_header  CVWL568.lib(drv_dsi_tx.o)
    0x00014c86   0x00014c86   0x0000006c   Code   RO         1812    i.drv_dsi_tx_command_mode_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x00014cf2   0x00014cf2   0x00000018   Code   RO         1814    i.drv_dsi_tx_config_eotp  CVWL568.lib(drv_dsi_tx.o)
    0x00014d0a   0x00014d0a   0x00000008   Code   RO         1815    i.drv_dsi_tx_config_int  CVWL568.lib(drv_dsi_tx.o)
    0x00014d12   0x00014d12   0x00000008   Code   RO         1816    i.drv_dsi_tx_dpi_lpcmd_time  CVWL568.lib(drv_dsi_tx.o)
    0x00014d1a   0x00014d1a   0x0000000a   Code   RO         1817    i.drv_dsi_tx_dpi_mode  CVWL568.lib(drv_dsi_tx.o)
    0x00014d24   0x00014d24   0x00000024   Code   RO         1818    i.drv_dsi_tx_dpi_polarity  CVWL568.lib(drv_dsi_tx.o)
    0x00014d48   0x00014d48   0x00000004   Code   RO         1819    i.drv_dsi_tx_edpi_cmd_size  CVWL568.lib(drv_dsi_tx.o)
    0x00014d4c   0x00014d4c   0x00000004   Code   RO         1821    i.drv_dsi_tx_get_cmd_status  CVWL568.lib(drv_dsi_tx.o)
    0x00014d50   0x00014d50   0x00000004   Code   RO         1823    i.drv_dsi_tx_mode   CVWL568.lib(drv_dsi_tx.o)
    0x00014d54   0x00014d54   0x00000018   Code   RO         1824    i.drv_dsi_tx_phy_clock_lane_auto_lp  CVWL568.lib(drv_dsi_tx.o)
    0x00014d6c   0x00014d6c   0x0000001a   Code   RO         1825    i.drv_dsi_tx_phy_clock_lane_req_hs  CVWL568.lib(drv_dsi_tx.o)
    0x00014d86   0x00014d86   0x0000000c   Code   RO         1827    i.drv_dsi_tx_phy_lane_mode  CVWL568.lib(drv_dsi_tx.o)
    0x00014d92   0x00014d92   0x00000064   Code   RO         1831    i.drv_dsi_tx_phy_status_ready  CVWL568.lib(drv_dsi_tx.o)
    0x00014df6   0x00014df6   0x0000003e   Code   RO         1832    i.drv_dsi_tx_phy_status_stopstate  CVWL568.lib(drv_dsi_tx.o)
    0x00014e34   0x00014e34   0x00000134   Code   RO         1834    i.drv_dsi_tx_phy_test_setup  CVWL568.lib(drv_dsi_tx.o)
    0x00014f68   0x00014f68   0x0000001e   Code   RO         1835    i.drv_dsi_tx_phy_time_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x00014f86   0x00014f86   0x00000008   Code   RO         1839    i.drv_dsi_tx_powerup  CVWL568.lib(drv_dsi_tx.o)
    0x00014f8e   0x00014f8e   0x0000001c   Code   RO         1840    i.drv_dsi_tx_response_mode  CVWL568.lib(drv_dsi_tx.o)
    0x00014faa   0x00014faa   0x00000018   Code   RO         1843    i.drv_dsi_tx_set_bta_ack  CVWL568.lib(drv_dsi_tx.o)
    0x00014fc2   0x00014fc2   0x0000000c   Code   RO         1844    i.drv_dsi_tx_set_esc_div  CVWL568.lib(drv_dsi_tx.o)
    0x00014fce   0x00014fce   0x00000002   PAD
    0x00014fd0   0x00014fd0   0x00000040   Code   RO         1845    i.drv_dsi_tx_set_int  CVWL568.lib(drv_dsi_tx.o)
    0x00015010   0x00015010   0x00000010   Code   RO         1846    i.drv_dsi_tx_set_time_out_div  CVWL568.lib(drv_dsi_tx.o)
    0x00015020   0x00015020   0x00000008   Code   RO         1847    i.drv_dsi_tx_set_video_chunk  CVWL568.lib(drv_dsi_tx.o)
    0x00015028   0x00015028   0x00000022   Code   RO         1848    i.drv_dsi_tx_set_video_timing  CVWL568.lib(drv_dsi_tx.o)
    0x0001504a   0x0001504a   0x00000008   Code   RO         1850    i.drv_dsi_tx_shutdown  CVWL568.lib(drv_dsi_tx.o)
    0x00015052   0x00015052   0x00000026   Code   RO         1851    i.drv_dsi_tx_timeout_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x00015078   0x00015078   0x000000aa   Code   RO         1854    i.drv_dsi_tx_video_mode_cfg  CVWL568.lib(drv_dsi_tx.o)
    0x00015122   0x00015122   0x00000016   Code   RO         1855    i.drv_dsi_tx_video_mode_disable_hact_cmd  CVWL568.lib(drv_dsi_tx.o)
    0x00015138   0x00015138   0x00000018   Code   RO         1856    i.drv_dsi_tx_video_mode_set_lp_cmd  CVWL568.lib(drv_dsi_tx.o)
    0x00015150   0x00015150   0x0000002e   Code   RO         2261    i.drv_efuse_enter_inactive  CVWL568.lib(drv_efuse.o)
    0x0001517e   0x0001517e   0x0000000c   Code   RO         2264    i.drv_efuse_int_enable  CVWL568.lib(drv_efuse.o)
    0x0001518a   0x0001518a   0x00000032   Code   RO         2265    i.drv_efuse_read    CVWL568.lib(drv_efuse.o)
    0x000151bc   0x000151bc   0x00000018   Code   RO         2266    i.drv_efuse_read_req  CVWL568.lib(drv_efuse.o)
    0x000151d4   0x000151d4   0x00000018   Code   RO         1465    i.drv_gpio_get_input_data  CVWL568.lib(drv_gpio.o)
    0x000151ec   0x000151ec   0x00000020   Code   RO         1471    i.drv_gpio_set_ioe  CVWL568.lib(drv_gpio.o)
    0x0001520c   0x0001520c   0x00000010   Code   RO         1472    i.drv_gpio_set_mode0  CVWL568.lib(drv_gpio.o)
    0x0001521c   0x0001521c   0x00000010   Code   RO         1473    i.drv_gpio_set_mode1  CVWL568.lib(drv_gpio.o)
    0x0001522c   0x0001522c   0x00000010   Code   RO         1474    i.drv_gpio_set_mode2  CVWL568.lib(drv_gpio.o)
    0x0001523c   0x0001523c   0x00000010   Code   RO         1475    i.drv_gpio_set_mode3  CVWL568.lib(drv_gpio.o)
    0x0001524c   0x0001524c   0x00000020   Code   RO          907    i.drv_gpio_set_output_data  CVWL568.lib(hal_gpio.o)
    0x0001526c   0x0001526c   0x00000130   Code   RO         1476    i.drv_gpio_set_pull_state  CVWL568.lib(drv_gpio.o)
    0x0001539c   0x0001539c   0x00000018   Code   RO         1923    i.drv_lcdc_config_bypass  CVWL568.lib(drv_lcdc.o)
    0x000153b4   0x000153b4   0x00000030   Code   RO         1924    i.drv_lcdc_config_ccm  CVWL568.lib(drv_lcdc.o)
    0x000153e4   0x000153e4   0x00000016   Code   RO         1925    i.drv_lcdc_config_disp_mode  CVWL568.lib(drv_lcdc.o)
    0x000153fa   0x000153fa   0x00000024   Code   RO         1926    i.drv_lcdc_config_dpi_polarity  CVWL568.lib(drv_lcdc.o)
    0x0001541e   0x0001541e   0x00000026   Code   RO         1927    i.drv_lcdc_config_dpi_timing  CVWL568.lib(drv_lcdc.o)
    0x00015444   0x00015444   0x00000016   Code   RO         1928    i.drv_lcdc_config_edpi_mode  CVWL568.lib(drv_lcdc.o)
    0x0001545a   0x0001545a   0x00000016   Code   RO         1929    i.drv_lcdc_config_endianness  CVWL568.lib(drv_lcdc.o)
    0x00015470   0x00015470   0x0000000c   Code   RO         1930    i.drv_lcdc_config_input_size  CVWL568.lib(drv_lcdc.o)
    0x0001547c   0x0001547c   0x0000001e   Code   RO         1931    i.drv_lcdc_config_int  CVWL568.lib(drv_lcdc.o)
    0x0001549a   0x0001549a   0x00000022   Code   RO         1932    i.drv_lcdc_config_int_single  CVWL568.lib(drv_lcdc.o)
    0x000154bc   0x000154bc   0x00000022   Code   RO         1933    i.drv_lcdc_config_overwrite  CVWL568.lib(drv_lcdc.o)
    0x000154de   0x000154de   0x0000000c   Code   RO         1934    i.drv_lcdc_config_overwrite_rgb  CVWL568.lib(drv_lcdc.o)
    0x000154ea   0x000154ea   0x0000001a   Code   RO         1935    i.drv_lcdc_config_partial_display_area  CVWL568.lib(drv_lcdc.o)
    0x00015504   0x00015504   0x00000022   Code   RO         1936    i.drv_lcdc_config_partial_display_enable  CVWL568.lib(drv_lcdc.o)
    0x00015526   0x00015526   0x0000001a   Code   RO         1938    i.drv_lcdc_config_scale_up_coef  CVWL568.lib(drv_lcdc.o)
    0x00015540   0x00015540   0x0000000c   Code   RO         1939    i.drv_lcdc_config_scale_up_step  CVWL568.lib(drv_lcdc.o)
    0x0001554c   0x0001554c   0x0000004c   Code   RO         1940    i.drv_lcdc_config_src_parameter  CVWL568.lib(drv_lcdc.o)
    0x00015598   0x00015598   0x00000006   Code   RO         1941    i.drv_lcdc_config_thresh  CVWL568.lib(drv_lcdc.o)
    0x0001559e   0x0001559e   0x00000012   Code   RO         1942    i.drv_lcdc_ctrl_flow  CVWL568.lib(drv_lcdc.o)
    0x000155b0   0x000155b0   0x00000020   Code   RO         1944    i.drv_lcdc_enable_shadow_reg  CVWL568.lib(drv_lcdc.o)
    0x000155d0   0x000155d0   0x00000040   Code   RO         1945    i.drv_lcdc_set_int  CVWL568.lib(drv_lcdc.o)
    0x00015610   0x00015610   0x00000018   Code   RO         1946    i.drv_lcdc_set_prefetch  CVWL568.lib(drv_lcdc.o)
    0x00015628   0x00015628   0x00000014   Code   RO         1947    i.drv_lcdc_set_video_hw_mode  CVWL568.lib(drv_lcdc.o)
    0x0001563c   0x0001563c   0x00000020   Code   RO         1948    i.drv_lcdc_start    CVWL568.lib(drv_lcdc.o)
    0x0001565c   0x0001565c   0x0000000c   Code   RO         1982    i.drv_memc_clear_status  CVWL568.lib(drv_memc.o)
    0x00015668   0x00015668   0x00000040   Code   RO         1983    i.drv_memc_enable_irq  CVWL568.lib(drv_memc.o)
    0x000156a8   0x000156a8   0x0000000c   Code   RO         1984    i.drv_memc_gen_a_tear_signal  CVWL568.lib(drv_memc.o)
    0x000156b4   0x000156b4   0x00000012   Code   RO         1985    i.drv_memc_get_status  CVWL568.lib(drv_memc.o)
    0x000156c6   0x000156c6   0x00000010   Code   RO         1986    i.drv_memc_rate_transfer_sel  CVWL568.lib(drv_memc.o)
    0x000156d6   0x000156d6   0x0000000e   Code   RO         1987    i.drv_memc_sel_vsync  CVWL568.lib(drv_memc.o)
    0x000156e4   0x000156e4   0x00000014   Code   RO         1988    i.drv_memc_set_active_height  CVWL568.lib(drv_memc.o)
    0x000156f8   0x000156f8   0x0000000c   Code   RO         1989    i.drv_memc_set_data_mode  CVWL568.lib(drv_memc.o)
    0x00015704   0x00015704   0x00000010   Code   RO         1992    i.drv_memc_set_double_buffer  CVWL568.lib(drv_memc.o)
    0x00015714   0x00015714   0x00000012   Code   RO         1993    i.drv_memc_set_double_buffer_reverse  CVWL568.lib(drv_memc.o)
    0x00015726   0x00015726   0x00000010   Code   RO         1995    i.drv_memc_set_fs_en_conditions  CVWL568.lib(drv_memc.o)
    0x00015736   0x00015736   0x00000014   Code   RO         1996    i.drv_memc_set_inten  CVWL568.lib(drv_memc.o)
    0x0001574a   0x0001574a   0x00000002   PAD
    0x0001574c   0x0001574c   0x00000018   Code   RO         1997    i.drv_memc_set_lcdc_st_conditions  CVWL568.lib(drv_memc.o)
    0x00015764   0x00015764   0x0000001a   Code   RO         1998    i.drv_memc_set_ltpo_mode  CVWL568.lib(drv_memc.o)
    0x0001577e   0x0001577e   0x0000000e   Code   RO         2002    i.drv_memc_set_tear_mode  CVWL568.lib(drv_memc.o)
    0x0001578c   0x0001578c   0x00000028   Code   RO         2003    i.drv_memc_set_tear_waveform  CVWL568.lib(drv_memc.o)
    0x000157b4   0x000157b4   0x0000000e   Code   RO         2005    i.drv_memc_set_vidc_sync_cnt  CVWL568.lib(drv_memc.o)
    0x000157c2   0x000157c2   0x00000002   PAD
    0x000157c4   0x000157c4   0x00000008   Code   RO         1594    i.drv_param_init_get_ccm  CVWL568.lib(drv_param_init.o)
    0x000157cc   0x000157cc   0x00000014   Code   RO         1595    i.drv_param_init_get_scld_filter_h  CVWL568.lib(drv_param_init.o)
    0x000157e0   0x000157e0   0x00000014   Code   RO         1596    i.drv_param_init_get_scld_filter_v  CVWL568.lib(drv_param_init.o)
    0x000157f4   0x000157f4   0x00000008   Code   RO         1597    i.drv_param_init_get_sclu_filter  CVWL568.lib(drv_param_init.o)
    0x000157fc   0x000157fc   0x00000014   Code   RO         1598    i.drv_param_init_set_ccm  CVWL568.lib(drv_param_init.o)
    0x00015810   0x00015810   0x00000064   Code   RO         1599    i.drv_param_init_set_scld_filter  CVWL568.lib(drv_param_init.o)
    0x00015874   0x00015874   0x00000024   Code   RO         1601    i.drv_param_p2r_filter_init  CVWL568.lib(drv_param_init.o)
    0x00015898   0x00015898   0x00000010   Code   RO         2282    i.drv_phy_enable_calibration  CVWL568.lib(drv_phy_common.o)
    0x000158a8   0x000158a8   0x0000003c   Code   RO         2283    i.drv_phy_get_calibration  CVWL568.lib(drv_phy_common.o)
    0x000158e4   0x000158e4   0x00000060   Code   RO         2284    i.drv_phy_get_pll_para  CVWL568.lib(drv_phy_common.o)
    0x00015944   0x00015944   0x00000054   Code   RO         2285    i.drv_phy_get_rate_para  CVWL568.lib(drv_phy_common.o)
    0x00015998   0x00015998   0x00000010   Code   RO         2286    i.drv_phy_test_clear  CVWL568.lib(drv_phy_common.o)
    0x000159a8   0x000159a8   0x00000018   Code   RO         2287    i.drv_phy_test_lock  CVWL568.lib(drv_phy_common.o)
    0x000159c0   0x000159c0   0x00000020   Code   RO         2289    i.drv_phy_test_write_1_byte  CVWL568.lib(drv_phy_common.o)
    0x000159e0   0x000159e0   0x00000026   Code   RO         2290    i.drv_phy_test_write_2_byte  CVWL568.lib(drv_phy_common.o)
    0x00015a06   0x00015a06   0x0000001e   Code   RO         2291    i.drv_phy_test_write_code  CVWL568.lib(drv_phy_common.o)
    0x00015a24   0x00015a24   0x00000020   Code   RO         2292    i.drv_phy_test_write_data  CVWL568.lib(drv_phy_common.o)
    0x00015a44   0x00015a44   0x00000018   Code   RO         1619    i.drv_pwr_set_pvd_mode  CVWL568.lib(drv_pwr.o)
    0x00015a5c   0x00015a5c   0x00000038   Code   RO         1620    i.drv_pwr_set_system_clk_src  CVWL568.lib(drv_pwr.o)
    0x00015a94   0x00015a94   0x0000000c   Code   RO         1773    i.drv_rx_phy_test_clear  CVWL568.lib(drv_dsi_rx.o)
    0x00015aa0   0x00015aa0   0x00000010   Code   RO         1774    i.drv_rx_phy_test_lock  CVWL568.lib(drv_dsi_rx.o)
    0x00015ab0   0x00015ab0   0x00000014   Code   RO         1776    i.drv_rx_phy_test_write_1_byte  CVWL568.lib(drv_dsi_rx.o)
    0x00015ac4   0x00015ac4   0x00000016   Code   RO         1777    i.drv_rx_phy_test_write_2_byte  CVWL568.lib(drv_dsi_rx.o)
    0x00015ada   0x00015ada   0x0000000a   Code   RO         2041    i.drv_rxbr_clear_pkt_buffer  CVWL568.lib(drv_rxbr.o)
    0x00015ae4   0x00015ae4   0x00000004   Code   RO         2042    i.drv_rxbr_clear_status0  CVWL568.lib(drv_rxbr.o)
    0x00015ae8   0x00015ae8   0x0000005a   Code   RO         2044    i.drv_rxbr_enable_irq  CVWL568.lib(drv_rxbr.o)
    0x00015b42   0x00015b42   0x00000002   PAD
    0x00015b44   0x00015b44   0x00000014   Code   RO         2045    i.drv_rxbr_frame_drop_cfg  CVWL568.lib(drv_rxbr.o)
    0x00015b58   0x00015b58   0x00000064   Code   RO         2046    i.drv_rxbr_get_clk  CVWL568.lib(drv_rxbr.o)
    0x00015bbc   0x00015bbc   0x00000004   Code   RO         2047    i.drv_rxbr_get_col_addr  CVWL568.lib(drv_rxbr.o)
    0x00015bc0   0x00015bc0   0x00000012   Code   RO         1109    i.drv_rxbr_get_int_source  CVWL568.lib(hal_internal_vsync.o)
    0x00015bd2   0x00015bd2   0x00000004   Code   RO         2050    i.drv_rxbr_get_page_addr  CVWL568.lib(drv_rxbr.o)
    0x00015bd6   0x00015bd6   0x0000000c   Code   RO         2052    i.drv_rxbr_get_pkt_buf_error_status  CVWL568.lib(drv_rxbr.o)
    0x00015be2   0x00015be2   0x00000012   Code   RO         1110    i.drv_rxbr_get_status0  CVWL568.lib(hal_internal_vsync.o)
    0x00015bf4   0x00015bf4   0x00000016   Code   RO         1111    i.drv_rxbr_get_status1  CVWL568.lib(hal_internal_vsync.o)
    0x00015c0a   0x00015c0a   0x0000000c   Code   RO         2053    i.drv_rxbr_hline_rcv0_cfg  CVWL568.lib(drv_rxbr.o)
    0x00015c16   0x00015c16   0x0000000c   Code   RO         2054    i.drv_rxbr_hline_rcv1_cfg  CVWL568.lib(drv_rxbr.o)
    0x00015c22   0x00015c22   0x00000008   Code   RO         2055    i.drv_rxbr_hline_rcv_cfg  CVWL568.lib(drv_rxbr.o)
    0x00015c2a   0x00015c2a   0x00000002   PAD
    0x00015c2c   0x00015c2c   0x0000000c   Code   RO         2056    i.drv_rxbr_register_irq0_callback  CVWL568.lib(drv_rxbr.o)
    0x00015c38   0x00015c38   0x0000000c   Code   RO         2057    i.drv_rxbr_register_irq1_callback  CVWL568.lib(drv_rxbr.o)
    0x00015c44   0x00015c44   0x00000014   Code   RO         2058    i.drv_rxbr_set_ack_pkt_header  CVWL568.lib(drv_rxbr.o)
    0x00015c58   0x00015c58   0x00000014   Code   RO         2061    i.drv_rxbr_set_color_format  CVWL568.lib(drv_rxbr.o)
    0x00015c6c   0x00015c6c   0x00000012   Code   RO         2063    i.drv_rxbr_set_filter_regs  CVWL568.lib(drv_rxbr.o)
    0x00015c7e   0x00015c7e   0x00000014   Code   RO         2064    i.drv_rxbr_set_inten  CVWL568.lib(drv_rxbr.o)
    0x00015c92   0x00015c92   0x00000010   Code   RO         2065    i.drv_rxbr_set_ltpo_drop_th  CVWL568.lib(drv_rxbr.o)
    0x00015ca2   0x00015ca2   0x00000026   Code   RO         2067    i.drv_rxbr_set_usr_cfg  CVWL568.lib(drv_rxbr.o)
    0x00015cc8   0x00015cc8   0x00000008   Code   RO         2068    i.drv_rxbr_set_usr_col  CVWL568.lib(drv_rxbr.o)
    0x00015cd0   0x00015cd0   0x00000008   Code   RO         2069    i.drv_rxbr_set_usr_row  CVWL568.lib(drv_rxbr.o)
    0x00015cd8   0x00015cd8   0x00000054   Code   RO         2562    i.drv_swire_set_int  CVWL568.lib(drv_swire.o)
    0x00015d2c   0x00015d2c   0x0000000c   Code   RO         1690    i.drv_sys_cfg_clear_all_int  CVWL568.lib(drv_sys_cfg.o)
    0x00015d38   0x00015d38   0x00000028   Code   RO         1691    i.drv_sys_cfg_clear_pending  CVWL568.lib(drv_sys_cfg.o)
    0x00015d60   0x00015d60   0x00000018   Code   RO         1694    i.drv_sys_cfg_sel_ap_rst_lvl_trig  CVWL568.lib(drv_sys_cfg.o)
    0x00015d78   0x00015d78   0x00000024   Code   RO         1701    i.drv_sys_cfg_set_int  CVWL568.lib(drv_sys_cfg.o)
    0x00015d9c   0x00015d9c   0x0000001a   Code   RO         2581    i.drv_timer_clear_status_flags  CVWL568.lib(drv_timer.o)
    0x00015db6   0x00015db6   0x00000020   Code   RO         2582    i.drv_timer_enable  CVWL568.lib(drv_timer.o)
    0x00015dd6   0x00015dd6   0x00000002   PAD
    0x00015dd8   0x00015dd8   0x00000010   Code   RO         2583    i.drv_timer_get_instance  CVWL568.lib(drv_timer.o)
    0x00015de8   0x00015de8   0x00000044   Code   RO         2586    i.drv_timer_handle_interrupt  CVWL568.lib(drv_timer.o)
    0x00015e2c   0x00015e2c   0x00000010   Code   RO         2588    i.drv_timer_set_compare_val  CVWL568.lib(drv_timer.o)
    0x00015e3c   0x00015e3c   0x00000054   Code   RO         2589    i.drv_timer_set_int  CVWL568.lib(drv_timer.o)
    0x00015e90   0x00015e90   0x0000000a   Code   RO         1857    i.drv_tx_phy_test_clear  CVWL568.lib(drv_dsi_tx.o)
    0x00015e9a   0x00015e9a   0x0000001c   Code   RO         1858    i.drv_tx_phy_test_enter  CVWL568.lib(drv_dsi_tx.o)
    0x00015eb6   0x00015eb6   0x0000001c   Code   RO         1859    i.drv_tx_phy_test_exit  CVWL568.lib(drv_dsi_tx.o)
    0x00015ed2   0x00015ed2   0x00000012   Code   RO         1861    i.drv_tx_phy_test_write_1_byte  CVWL568.lib(drv_dsi_tx.o)
    0x00015ee4   0x00015ee4   0x00000014   Code   RO         1862    i.drv_tx_phy_test_write_2_byte  CVWL568.lib(drv_dsi_tx.o)
    0x00015ef8   0x00015ef8   0x00000010   Code   RO         1863    i.drv_tx_phy_test_write_code  CVWL568.lib(drv_dsi_tx.o)
    0x00015f08   0x00015f08   0x00000008   Code   RO         2111    i.drv_vidc_clear_irq  CVWL568.lib(drv_vidc.o)
    0x00015f10   0x00015f10   0x00000018   Code   RO         2115    i.drv_vidc_enable   CVWL568.lib(drv_vidc.o)
    0x00015f28   0x00015f28   0x00000040   Code   RO         2116    i.drv_vidc_enable_irq  CVWL568.lib(drv_vidc.o)
    0x00015f68   0x00015f68   0x00000012   Code   RO         2118    i.drv_vidc_get_irq_status  CVWL568.lib(drv_vidc.o)
    0x00015f7a   0x00015f7a   0x00000002   PAD
    0x00015f7c   0x00015f7c   0x00000028   Code   RO         2122    i.drv_vidc_init_module_enable  CVWL568.lib(drv_vidc.o)
    0x00015fa4   0x00015fa4   0x0000000c   Code   RO         2123    i.drv_vidc_register_callback  CVWL568.lib(drv_vidc.o)
    0x00015fb0   0x00015fb0   0x00000006   Code   RO         2124    i.drv_vidc_reset    CVWL568.lib(drv_vidc.o)
    0x00015fb6   0x00015fb6   0x0000003c   Code   RO         2126    i.drv_vidc_set_dst_parameter  CVWL568.lib(drv_vidc.o)
    0x00015ff2   0x00015ff2   0x00000014   Code   RO         2130    i.drv_vidc_set_irqen  CVWL568.lib(drv_vidc.o)
    0x00016006   0x00016006   0x00000010   Code   RO         2131    i.drv_vidc_set_mirror  CVWL568.lib(drv_vidc.o)
    0x00016016   0x00016016   0x00000008   Code   RO         2134    i.drv_vidc_set_p2r_hcoef0  CVWL568.lib(drv_vidc.o)
    0x0001601e   0x0001601e   0x00000026   Code   RO         2135    i.drv_vidc_set_p2r_hinitb  CVWL568.lib(drv_vidc.o)
    0x00016044   0x00016044   0x00000026   Code   RO         2136    i.drv_vidc_set_p2r_hinitr  CVWL568.lib(drv_vidc.o)
    0x0001606a   0x0001606a   0x00000002   PAD
    0x0001606c   0x0001606c   0x00000018   Code   RO         2137    i.drv_vidc_set_pentile_swap  CVWL568.lib(drv_vidc.o)
    0x00016084   0x00016084   0x0000000a   Code   RO         2138    i.drv_vidc_set_pu_ctrl  CVWL568.lib(drv_vidc.o)
    0x0001608e   0x0001608e   0x00000010   Code   RO         2139    i.drv_vidc_set_rotation  CVWL568.lib(drv_vidc.o)
    0x0001609e   0x0001609e   0x0000000a   Code   RO         2140    i.drv_vidc_set_scld_hcoef0  CVWL568.lib(drv_vidc.o)
    0x000160a8   0x000160a8   0x0000000a   Code   RO         2141    i.drv_vidc_set_scld_hcoef1  CVWL568.lib(drv_vidc.o)
    0x000160b2   0x000160b2   0x00000012   Code   RO         2142    i.drv_vidc_set_scld_step  CVWL568.lib(drv_vidc.o)
    0x000160c4   0x000160c4   0x0000000a   Code   RO         2143    i.drv_vidc_set_scld_vcoef0  CVWL568.lib(drv_vidc.o)
    0x000160ce   0x000160ce   0x0000000a   Code   RO         2144    i.drv_vidc_set_scld_vcoef1  CVWL568.lib(drv_vidc.o)
    0x000160d8   0x000160d8   0x00000016   Code   RO         2145    i.drv_vidc_set_src_parameter  CVWL568.lib(drv_vidc.o)
    0x000160ee   0x000160ee   0x00000002   PAD
    0x000160f0   0x000160f0   0x00000010   Code   RO         2700    i.drv_wdg_clear_counter  CVWL568.lib(drv_wdg.o)
    0x00016100   0x00016100   0x00000010   Code   RO         2701    i.drv_wdg_clear_edge_flag  CVWL568.lib(drv_wdg.o)
    0x00016110   0x00016110   0x00000010   Code   RO         2704    i.drv_wdg_read_edge_flag  CVWL568.lib(drv_wdg.o)
    0x00016120   0x00016120   0x00000040   Code   RO         2707    i.drv_wdg_set_int   CVWL568.lib(drv_wdg.o)
    0x00016160   0x00016160   0x0000000a   Code   RO         1377    i.fls_clr_interrupt_flag  CVWL568.lib(drv_fls.o)
    0x0001616a   0x0001616a   0x00000014   Code   RO         1076    i.fputc             CVWL568.lib(tau_log.o)
    0x0001617e   0x0001617e   0x00000002   PAD
    0x00016180   0x00016180   0x00000050   Code   RO          115    i.frame_start_cb    ap_demo.o
    0x000161d0   0x000161d0   0x00000034   Code   RO          706    i.hal_dsi_rx_ctrl_create_handle  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016204   0x00016204   0x00000028   Code   RO          710    i.hal_dsi_rx_ctrl_dsc_async_handler  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001622c   0x0001622c   0x00000028   Code   RO          712    i.hal_dsi_rx_ctrl_gen_a_tear_signal  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016254   0x00016254   0x00000028   Code   RO          714    i.hal_dsi_rx_ctrl_get_max_ret_size  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001627c   0x0001627c   0x00000098   Code   RO          716    i.hal_dsi_rx_ctrl_init  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016314   0x00016314   0x000001a4   Code   RO          717    i.hal_dsi_rx_ctrl_init_clk  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000164b8   0x000164b8   0x000000d8   Code   RO          718    i.hal_dsi_rx_ctrl_init_dsi_rx  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016590   0x00016590   0x00000160   Code   RO          719    i.hal_dsi_rx_ctrl_init_memc  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x000166f0   0x000166f0   0x00000150   Code   RO          720    i.hal_dsi_rx_ctrl_init_rxbr  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016840   0x00016840   0x0000022c   Code   RO          721    i.hal_dsi_rx_ctrl_init_vidc  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016a6c   0x00016a6c   0x0000003c   Code   RO          722    i.hal_dsi_rx_ctrl_pre_init_pps  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016aa8   0x00016aa8   0x00000050   Code   RO          725    i.hal_dsi_rx_ctrl_restart  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016af8   0x00016af8   0x000000f0   Code   RO          726    i.hal_dsi_rx_ctrl_send_ack_cmd  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016be8   0x00016be8   0x0000002c   Code   RO          728    i.hal_dsi_rx_ctrl_set_cus_esc_clk  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016c14   0x00016c14   0x0000006c   Code   RO          729    i.hal_dsi_rx_ctrl_set_cus_scld_filter  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016c80   0x00016c80   0x00000034   Code   RO          730    i.hal_dsi_rx_ctrl_set_cus_sync_line  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016cb4   0x00016cb4   0x00000038   Code   RO          734    i.hal_dsi_rx_ctrl_set_ipi_cfg  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016cec   0x00016cec   0x00000072   Code   RO          739    i.hal_dsi_rx_ctrl_set_rxbr_clk  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016d5e   0x00016d5e   0x0000000e   Code   RO          742    i.hal_dsi_rx_ctrl_set_tear_mode_ex  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016d6c   0x00016d6c   0x0000003c   Code   RO          743    i.hal_dsi_rx_ctrl_start  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016da8   0x00016da8   0x00000020   Code   RO          746    i.hal_dsi_rx_ctrl_toggle_resolution  CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00016dc8   0x00016dc8   0x00000190   Code   RO          801    i.hal_dsi_tx_calc_video_chunks  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00016f58   0x00016f58   0x00000034   Code   RO          802    i.hal_dsi_tx_config_params_for_lane_rate  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00016f8c   0x00016f8c   0x00000428   Code   RO          803    i.hal_dsi_tx_count_lane_rate  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000173b4   0x000173b4   0x0000002c   Code   RO          806    i.hal_dsi_tx_ctrl_create_handle  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000173e0   0x000173e0   0x0000004c   Code   RO          811    i.hal_dsi_tx_ctrl_enter_init_panel_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001742c   0x0001742c   0x00000028   Code   RO          813    i.hal_dsi_tx_ctrl_exit_init_panel_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017454   0x00017454   0x000000a4   Code   RO          815    i.hal_dsi_tx_ctrl_init  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000174f8   0x000174f8   0x00000024   Code   RO          816    i.hal_dsi_tx_ctrl_init_clk  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001751c   0x0001751c   0x0000000c   Code   RO          817    i.hal_dsi_tx_ctrl_panel_reset_pin  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017528   0x00017528   0x00000020   Code   RO          820    i.hal_dsi_tx_ctrl_set_ccm  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017548   0x00017548   0x00000014   Code   RO          826    i.hal_dsi_tx_ctrl_set_overwrite_rgb  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001755c   0x0001755c   0x00000010   Code   RO          827    i.hal_dsi_tx_ctrl_set_partial_disp  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001756c   0x0001756c   0x00000024   Code   RO          828    i.hal_dsi_tx_ctrl_set_partial_disp_area  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017590   0x00017590   0x000000a8   Code   RO          831    i.hal_dsi_tx_ctrl_start  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017638   0x00017638   0x000000f0   Code   RO          833    i.hal_dsi_tx_ctrl_write_array_cmd  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017728   0x00017728   0x000000cc   Code   RO          834    i.hal_dsi_tx_ctrl_write_cmd  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000177f4   0x000177f4   0x00000044   Code   RO          835    i.hal_dsi_tx_init_data_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017838   0x00017838   0x00000030   Code   RO          836    i.hal_dsi_tx_init_dpi_cfg  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017868   0x00017868   0x00000020   Code   RO          837    i.hal_dsi_tx_init_interrupt  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017888   0x00017888   0x00000020   Code   RO          838    i.hal_dsi_tx_init_phy_cfg  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000178a8   0x000178a8   0x00000094   Code   RO          839    i.hal_dsi_tx_init_remains  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001793c   0x0001793c   0x00000058   Code   RO          840    i.hal_dsi_tx_init_video_mode  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00017994   0x00017994   0x00000044   Code   RO          841    i.hal_dsi_tx_send_cmd  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000179d8   0x000179d8   0x00000012   Code   RO          909    i.hal_gpio_get_input_data  CVWL568.lib(hal_gpio.o)
    0x000179ea   0x000179ea   0x00000002   PAD
    0x000179ec   0x000179ec   0x00000020   Code   RO          913    i.hal_gpio_init_input  CVWL568.lib(hal_gpio.o)
    0x00017a0c   0x00017a0c   0x00000028   Code   RO          914    i.hal_gpio_init_output  CVWL568.lib(hal_gpio.o)
    0x00017a34   0x00017a34   0x00000060   Code   RO          918    i.hal_gpio_set_mode  CVWL568.lib(hal_gpio.o)
    0x00017a94   0x00017a94   0x00000008   Code   RO          919    i.hal_gpio_set_output_data  CVWL568.lib(hal_gpio.o)
    0x00017a9c   0x00017a9c   0x00000020   Code   RO          921    i.hal_gpio_set_pull_state  CVWL568.lib(hal_gpio.o)
    0x00017abc   0x00017abc   0x00000018   Code   RO         1112    i.hal_internal_check_video_auto_sync  CVWL568.lib(hal_internal_vsync.o)
    0x00017ad4   0x00017ad4   0x000000fc   Code   RO         1113    i.hal_internal_init_memc  CVWL568.lib(hal_internal_vsync.o)
    0x00017bd0   0x00017bd0   0x0000002a   Code   RO         1114    i.hal_internal_rx_dcs_async_handler  CVWL568.lib(hal_internal_vsync.o)
    0x00017bfa   0x00017bfa   0x00000002   PAD
    0x00017bfc   0x00017bfc   0x00000058   Code   RO         1115    i.hal_internal_rx_dcs_polling  CVWL568.lib(hal_internal_vsync.o)
    0x00017c54   0x00017c54   0x00000010   Code   RO         1117    i.hal_internal_sync_get_fb_setting  CVWL568.lib(hal_internal_vsync.o)
    0x00017c64   0x00017c64   0x00000010   Code   RO         1118    i.hal_internal_sync_get_hight_performan_mode  CVWL568.lib(hal_internal_vsync.o)
    0x00017c74   0x00017c74   0x0000022c   Code   RO         1119    i.hal_internal_sync_input_resolution_change  CVWL568.lib(hal_internal_vsync.o)
    0x00017ea0   0x00017ea0   0x00000028   Code   RO         1122    i.hal_internal_vsync_deinit  CVWL568.lib(hal_internal_vsync.o)
    0x00017ec8   0x00017ec8   0x00000018   Code   RO         1124    i.hal_internal_vsync_get_sync_line  CVWL568.lib(hal_internal_vsync.o)
    0x00017ee0   0x00017ee0   0x0000000c   Code   RO         1125    i.hal_internal_vsync_get_tear_mode  CVWL568.lib(hal_internal_vsync.o)
    0x00017eec   0x00017eec   0x0000000c   Code   RO         1126    i.hal_internal_vsync_get_tx_state  CVWL568.lib(hal_internal_vsync.o)
    0x00017ef8   0x00017ef8   0x00000140   Code   RO         1127    i.hal_internal_vsync_init_rx  CVWL568.lib(hal_internal_vsync.o)
    0x00018038   0x00018038   0x000000b0   Code   RO         1128    i.hal_internal_vsync_init_tx  CVWL568.lib(hal_internal_vsync.o)
    0x000180e8   0x000180e8   0x00000090   Code   RO         1130    i.hal_internal_vsync_set_auto_hw_filter  CVWL568.lib(hal_internal_vsync.o)
    0x00018178   0x00018178   0x00000024   Code   RO         1132    i.hal_internal_vsync_set_rx_state  CVWL568.lib(hal_internal_vsync.o)
    0x0001819c   0x0001819c   0x00000044   Code   RO         1133    i.hal_internal_vsync_set_sync_line  CVWL568.lib(hal_internal_vsync.o)
    0x000181e0   0x000181e0   0x00000050   Code   RO         1134    i.hal_internal_vsync_set_tear_mode  CVWL568.lib(hal_internal_vsync.o)
    0x00018230   0x00018230   0x00000084   Code   RO         1135    i.hal_internal_vsync_set_tx_state  CVWL568.lib(hal_internal_vsync.o)
    0x000182b4   0x000182b4   0x00000010   Code   RO         1721    i.hal_intl_svs_deinit_tx  CVWL568.lib(hal_internal_soft_sync.o)
    0x000182c4   0x000182c4   0x00000024   Code   RO         1722    i.hal_intl_svs_handle  CVWL568.lib(hal_internal_soft_sync.o)
    0x000182e8   0x000182e8   0x00000078   Code   RO         1723    i.hal_intl_svs_init_rx  CVWL568.lib(hal_internal_soft_sync.o)
    0x00018360   0x00018360   0x00000014   Code   RO         1724    i.hal_intl_svs_init_tx  CVWL568.lib(hal_internal_soft_sync.o)
    0x00018374   0x00018374   0x0000000c   Code   RO         1726    i.hal_intl_svs_set_sync_coef  CVWL568.lib(hal_internal_soft_sync.o)
    0x00018380   0x00018380   0x00000048   Code   RO         1727    i.hal_intl_svs_update_rxbr_clk  CVWL568.lib(hal_internal_soft_sync.o)
    0x000183c8   0x000183c8   0x00000024   Code   RO          842    i.hal_lcdc_config_ccm  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000183ec   0x000183ec   0x00000064   Code   RO          843    i.hal_lcdc_config_remains  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018450   0x00018450   0x00000014   Code   RO          844    i.hal_lcdc_config_rgb_to_pentile  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018464   0x00018464   0x00000164   Code   RO          845    i.hal_lcdc_config_upscaler  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000185c8   0x000185c8   0x00000054   Code   RO          846    i.hal_lcdc_init_cfg  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001861c   0x0001861c   0x000001cc   Code   RO          847    i.hal_lcdc_init_clk  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x000187e8   0x000187e8   0x00000040   Code   RO          848    i.hal_lcdc_init_interrupt  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018828   0x00018828   0x00000008   Code   RO         1033    i.hal_system_enable_systick  CVWL568.lib(hal_system.o)
    0x00018830   0x00018830   0x00000008   Code   RO         1035    i.hal_system_get_tick  CVWL568.lib(hal_system.o)
    0x00018838   0x00018838   0x00000088   Code   RO         1037    i.hal_system_init   CVWL568.lib(hal_system.o)
    0x000188c0   0x000188c0   0x0000001c   Code   RO         1038    i.hal_system_init_console  CVWL568.lib(hal_system.o)
    0x000188dc   0x000188dc   0x00000008   Code   RO         1041    i.hal_system_set_phy_calibration  CVWL568.lib(hal_system.o)
    0x000188e4   0x000188e4   0x00000030   Code   RO          849    i.hal_tx_frame_rate_adjust  CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00018914   0x00018914   0x0000008c   Code   RO         1087    i.hal_uart_init     CVWL568.lib(hal_uart.o)
    0x000189a0   0x000189a0   0x00000010   Code   RO         1090    i.hal_uart_transmit_blocking  CVWL568.lib(hal_uart.o)
    0x000189b0   0x000189b0   0x00000110   Code   RO         2221    i.handle_init       CVWL568.lib(irq_redirect .o)
    0x00018ac0   0x00018ac0   0x0000006c   Code   RO          116    i.init_mipi_tx      ap_demo.o
    0x00018b2c   0x00018b2c   0x000000a0   Code   RO          117    i.init_panel        ap_demo.o
    0x00018bcc   0x00018bcc   0x0000000a   Code   RO            3    i.main              main.o
    0x00018bd6   0x00018bd6   0x00000002   PAD
    0x00018bd8   0x00018bd8   0x000000d4   Code   RO          118    i.open_mipi_rx      ap_demo.o
    0x00018cac   0x00018cac   0x0000009c   Code   RO          119    i.pps_update_handle  ap_demo.o
    0x00018d48   0x00018d48   0x000003f4   Code   RO         1139    i.rx_get_dcs_packet_data  CVWL568.lib(hal_internal_vsync.o)
    0x0001913c   0x0001913c   0x0000016c   Code   RO         1140    i.rx_partial_update  CVWL568.lib(hal_internal_vsync.o)
    0x000192a8   0x000192a8   0x0000008c   Code   RO         1141    i.rx_receive_packet  CVWL568.lib(hal_internal_vsync.o)
    0x00019334   0x00019334   0x00000180   Code   RO         1142    i.rx_receive_pps    CVWL568.lib(hal_internal_vsync.o)
    0x000194b4   0x000194b4   0x000000cc   Code   RO         1143    i.rxbr_irq0_callback  CVWL568.lib(hal_internal_vsync.o)
    0x00019580   0x00019580   0x00000244   Code   RO         1144    i.rxbr_irq1_callback  CVWL568.lib(hal_internal_vsync.o)
    0x000197c4   0x000197c4   0x000000c4   Code   RO         1145    i.soft_gen_te       CVWL568.lib(hal_internal_vsync.o)
    0x00019888   0x00019888   0x000000c0   Code   RO         1146    i.soft_gen_te_double_buffer  CVWL568.lib(hal_internal_vsync.o)
    0x00019948   0x00019948   0x00000048   Code   RO         2738    i.sqrt              m_ps.l(sqrt.o)
    0x00019990   0x00019990   0x000000ac   Code   RO         1728    i.svs_direct_mode_setting  CVWL568.lib(hal_internal_soft_sync.o)
    0x00019a3c   0x00019a3c   0x0000001c   Code   RO         1729    i.svs_get_rel_intv  CVWL568.lib(hal_internal_soft_sync.o)
    0x00019a58   0x00019a58   0x000000b0   Code   RO         1730    i.svs_sync_handle   CVWL568.lib(hal_internal_soft_sync.o)
    0x00019b08   0x00019b08   0x000000f4   Code   RO         1731    i.svs_wait_start    CVWL568.lib(hal_internal_soft_sync.o)
    0x00019bfc   0x00019bfc   0x000000d8   Code   RO         1732    i.svs_waite_fr_stab  CVWL568.lib(hal_internal_soft_sync.o)
    0x00019cd4   0x00019cd4   0x00000108   Code   RO         1147    i.vidc_callback     CVWL568.lib(hal_internal_vsync.o)
    0x00019ddc   0x00019ddc   0x000000d8   Code   RO         1148    i.vpre_err_reset    CVWL568.lib(hal_internal_vsync.o)
    0x00019eb4   0x00019eb4   0x000001cc   Code   RO         1149    i.vsync_set_te_mode  CVWL568.lib(hal_internal_vsync.o)
    0x0001a080   0x0001a080   0x00001f74   Data   RO          123    .constdata          ap_demo.o
    0x0001bff4   0x0001bff4   0x000000d2   Data   RO          924    .constdata          CVWL568.lib(hal_gpio.o)
    0x0001c0c6   0x0001c0c6   0x00000002   PAD
    0x0001c0c8   0x0001c0c8   0x00000008   Data   RO         1602    .constdata          CVWL568.lib(drv_param_init.o)
    0x0001c0d0   0x0001c0d0   0x00000186   Data   RO         2293    .constdata          CVWL568.lib(drv_phy_common.o)
    0x0001c256   0x0001c256   0x00000002   PAD
    0x0001c258   0x0001c258   0x00000048   Data   RO          749    .conststring        CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x0001c2a0   0x0001c2a0   0x00000043   Data   RO          852    .conststring        CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x0001c2e3   0x0001c2e3   0x00000001   PAD
    0x0001c2e4   0x0001c2e4   0x00000178   Data   RO         1151    .conststring        CVWL568.lib(hal_internal_vsync.o)
    0x0001c45c   0x0001c45c   0x00000030   Data   RO         3102    Region$$Table       anon$$obj.o


    Execution Region RW_RAM1 (Exec base: 0x00070000, Load base: 0x0001c48c, Size: 0x00000000, Max: 0x000000f0, ABSOLUTE)

    **** No section assigned to this execution region ****


    Execution Region RW_RAM2 (Exec base: 0x00070100, Load base: 0x0001c48c, Size: 0x000000c0, Max: 0x000000d0, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00070100        -       0x000000c0   Zero   RW         2222    .ARM.__AT_0x00070100  CVWL568.lib(irq_redirect .o)


    Execution Region RW_RAM3 (Exec base: 0x000701d0, Load base: 0x0001c48c, Size: 0x00003658, Max: 0x00007e30, ABSOLUTE, COMPRESSED[0x0000052c])

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x000701d0   COMPRESSED   0x00000238   Data   RW          124    .data               ap_demo.o
    0x00070408   COMPRESSED   0x0000003b   Data   RW          441    .data               app_tp_st_touch.o
    0x00070443   COMPRESSED   0x00000001   PAD
    0x00070444   COMPRESSED   0x000000e4   Data   RW          593    .data               WL568_S21_NT37701_TP.lib(app_tp_for_custom_s8.o)
    0x00070528   COMPRESSED   0x00000008   Data   RW          750    .data               CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00070530   COMPRESSED   0x00000003   Data   RW          853    .data               CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00070533   COMPRESSED   0x00000001   PAD
    0x00070534   COMPRESSED   0x00000018   Data   RW         1152    .data               CVWL568.lib(hal_internal_vsync.o)
    0x0007054c   COMPRESSED   0x0000000c   Data   RW         1213    .data               CVWL568.lib(drv_common.o)
    0x00070558   COMPRESSED   0x00000004   Data   RW         1480    .data               CVWL568.lib(drv_gpio.o)
    0x0007055c   COMPRESSED   0x00000004   Data   RW         1547    .data               CVWL568.lib(drv_i2c_master.o)
    0x00070560   COMPRESSED   0x00000004   Data   RW         1578    .data               CVWL568.lib(drv_i2c_slave.o)
    0x00070564   COMPRESSED   0x000004a4   Data   RW         1603    .data               CVWL568.lib(drv_param_init.o)
    0x00070a08   COMPRESSED   0x00000004   Data   RW         1670    .data               CVWL568.lib(drv_spi_master.o)
    0x00070a0c   COMPRESSED   0x00000001   Data   RW         1702    .data               CVWL568.lib(drv_sys_cfg.o)
    0x00070a0d   COMPRESSED   0x00000003   PAD
    0x00070a10   COMPRESSED   0x00000008   Data   RW         2071    .data               CVWL568.lib(drv_rxbr.o)
    0x00070a18   COMPRESSED   0x00000004   Data   RW         2147    .data               CVWL568.lib(drv_vidc.o)
    0x00070a1c   COMPRESSED   0x00000001   Data   RW         2294    .data               CVWL568.lib(drv_phy_common.o)
    0x00070a1d   COMPRESSED   0x00000003   PAD
    0x00070a20   COMPRESSED   0x0000000c   Data   RW         2314    .data               CVWL568.lib(drv_chip_info.o)
    0x00070a2c   COMPRESSED   0x00000012   Data   RW         2423    .data               CVWL568.lib(norflash.o)
    0x00070a3e   COMPRESSED   0x00000002   PAD
    0x00070a40   COMPRESSED   0x0000000c   Data   RW         2510    .data               CVWL568.lib(drv_pwm.o)
    0x00070a4c   COMPRESSED   0x00000008   Data   RW         2565    .data               CVWL568.lib(drv_swire.o)
    0x00070a54   COMPRESSED   0x00000050   Data   RW         2592    .data               CVWL568.lib(drv_timer.o)
    0x00070aa4   COMPRESSED   0x00000008   Data   RW         2642    .data               CVWL568.lib(drv_uart.o)
    0x00070aac   COMPRESSED   0x0000000c   Data   RW         2709    .data               CVWL568.lib(drv_wdg.o)
    0x00070ab8   COMPRESSED   0x00000004   Data   RW         3071    .data               mc_p.l(stdout.o)
    0x00070abc   COMPRESSED   0x00000004   Data   RW         3083    .data               mc_p.l(errno.o)
    0x00070ac0        -       0x00000024   Zero   RW          122    .bss                ap_demo.o
    0x00070ae4        -       0x000000c4   Zero   RW          748    .bss                CVWL568.lib(hal_dsi_rx_ctrl.o)
    0x00070ba8        -       0x0000004c   Zero   RW          850    .bss                CVWL568.lib(hal_dsi_tx_ctrl.o)
    0x00070bf4        -       0x00000100   Zero   RW         1077    .bss                CVWL568.lib(tau_log.o)
    0x00070cf4        -       0x000000d0   Zero   RW         1092    .bss                CVWL568.lib(hal_uart.o)
    0x00070dc4        -       0x00000974   Zero   RW         1150    .bss                CVWL568.lib(hal_internal_vsync.o)
    0x00071738        -       0x0000001c   Zero   RW         1342    .bss                CVWL568.lib(drv_dma.o)
    0x00071754        -       0x00000040   Zero   RW         1479    .bss                CVWL568.lib(drv_gpio.o)
    0x00071794        -       0x00000040   Zero   RW         1733    .bss                CVWL568.lib(hal_internal_soft_sync.o)
    0x000717d4        -       0x00000020   Zero   RW         2358    .bss                CVWL568.lib(hal_spi_slave.o)
    0x000717f4        -       0x00001030   Zero   RW         2727    .bss                CVWL568.lib(dcs_packet_fifo.o)
    0x00072824   COMPRESSED   0x00000004   PAD
    0x00072828        -       0x00001000   Zero   RW          565    STACK               startup_armcm0.o


==============================================================================

Image component sizes


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Object Name

      6142        688       8052        568         36      29155   ap_demo.o
        32          4          0         59          0       4572   app_tp_st_touch.o
        36          6          0          0          0        565   board.o
        10          0          0          0          0       5715   main.o
       120         18        192          0       4096       2120   startup_armcm0.o

    ----------------------------------------------------------------------
      6344        716       8292        628       4132      42127   Object Totals
         0          0         48          0          0          0   (incl. Generated)
         4          0          0          1          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Member Name

       216         32          0          0       4144        252   dcs_packet_fifo.o
       272         96          0         12          0        256   drv_chip_info.o
       204         88         24         12          0        324   drv_common.o
       420         90          0          0          0       1200   drv_crgu.o
       196         12          0          0         28        272   drv_dma.o
       232         28          0          0          0        340   drv_dsc_dec.o
      1658        494          0          0          0       1396   drv_dsi_rx.o
      1528        118          0          0          0       2428   drv_dsi_tx.o
       132          0          0          0          0        256   drv_efuse.o
        10          0          0          0          0         60   drv_fls.o
       684         94          0          4         64       1044   drv_gpio.o
        16          8          0          4          0         60   drv_i2c_master.o
        24         10          0          4          0         60   drv_i2c_slave.o
       704          6          0          0          0       1504   drv_lcdc.o
       492         28          0          0          0       1112   drv_memc.o
       212         44          8       1188          0        452   drv_param_init.o
       428         30        390          1          0        664   drv_phy_common.o
        72         10          0         12          0         76   drv_pwm.o
        80         18          0          0          0        120   drv_pwr.o
       560         74          0          8          0       1560   drv_rxbr.o
        72         20          0          4          0        128   drv_spi_master.o
       116         12          0          8          0        140   drv_swire.o
       168         34          0          1          0        320   drv_sys_cfg.o
       282         16          0         80          0        680   drv_timer.o
       698         18          0          8          0        680   drv_uart.o
       510         28          0          4          0       1452   drv_vidc.o
       168         22          0         12          0        316   drv_wdg.o
      3090        294         72          8        196       1620   hal_dsi_rx_ctrl.o
      4256        288         67          3         76       2336   hal_dsi_tx_ctrl.o
       258         28        210          0          0        468   hal_gpio.o
      1112        188          0          0         64        776   hal_internal_soft_sync.o
      8052       1622        376         24       2420       2680   hal_internal_vsync.o
       580         32          0          0         32        136   hal_spi_slave.o
       188         32          0          0          0        340   hal_system.o
       156         18          0          0        208        144   hal_uart.o
      1076        324          0          0        192       1980   irq_redirect .o
        48         10          0         18          0         68   norflash.o
        58          0          0          0          0        128   tau_delay.o
        60         10          0          0        256        156   tau_log.o
         0          0          0        228          0      15807   app_tp_for_custom_s8.o
       200         20          0          0          0         76   ceil.o
        72          6          0          0          0         76   sqrt.o
        86          0          0          0          0          0   __dczerorl2.o
         0          0          0          0          0          0   entry.o
         0          0          0          0          0          0   entry10a.o
         0          0          0          0          0          0   entry11a.o
         8          4          0          0          0          0   entry2.o
         4          0          0          0          0          0   entry5.o
         0          0          0          0          0          0   entry7b.o
         0          0          0          0          0          0   entry8b.o
         8          4          0          0          0          0   entry9a.o
        12          6          0          4          0         60   errno.o
        30          0          0          0          0          0   handlers.o
        40          0          0          0          0         72   idiv.o
        36          8          0          0          0         68   init.o
         0          0          0          0          0          0   iusefp.o
        32          0          0          0          0         68   llshl.o
        38          0          0          0          0         68   llsshr.o
        34          0          0          0          0         68   llushr.o
        36          0          0          0          0         60   memcpya.o
        36          0          0          0          0        100   memseta.o
      2298        104          0          0          0        544   printfa.o
         0          0          0          4          0          0   stdout.o
        44          0          0          0          0         72   uidiv.o
        96          0          0          0          0         84   uldiv.o
        40          2          0          0          0         68   cdcmple.o
        40          2          0          0          0         68   cdrcmple.o
        20          0          0          0          0         68   cfcmple.o
        20          0          0          0          0         68   cfrcmple.o
       356          4          0          0          0        140   dadd.o
       240          6          0          0          0         84   ddiv.o
       236          0          0          0          0        216   depilogue.o
        72         10          0          0          0         72   dfixi.o
        60         10          0          0          0         68   dfixui.o
        64         10          0          0          0         68   dfixul.o
        28          4          0          0          0         68   dfltui.o
       208          6          0          0          0         88   dmul.o
       162          0          0          0          0         80   dsqrt.o
        40          0          0          0          0         60   f2d.o
       178          0          0          0          0        108   fadd.o
       124          0          0          0          0         72   fdiv.o
       130          0          0          0          0        144   fepilogue.o
        50          0          0          0          0         60   ffixi.o
        40          0          0          0          0         60   ffixui.o
        22          0          0          0          0         68   fflti.o
        14          0          0          0          0         68   ffltui.o
       122          0          0          0          0         72   fmul.o
        24          0          0          0          0         60   fscalb.o

    ----------------------------------------------------------------------
     34528       4482       1152       1660       7684      47135   Library Totals
        40          0          5          9          4          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Name

     29088       4276       1147       1415       7680      27984   CVWL568.lib
         0          0          0        228          0      15807   WL568_S21_NT37701_TP.lib
       272         26          0          0          0        152   m_ps.l
      2838        126          0          8          0       1264   mc_p.l
      2290         54          0          0          0       1928   mf_p.l

    ----------------------------------------------------------------------
     34528       4482       1152       1660       7684      47135   Library Totals

    ----------------------------------------------------------------------

==============================================================================


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   

     40872       5198       9444       2288      11816      68378   Grand Totals
     40872       5198       9444       1324      11816      68378   ELF Image Totals (compressed)
     40872       5198       9444       1324          0          0   ROM Totals

==============================================================================

    Total RO  Size (Code + RO Data)                50316 (  49.14kB)
    Total RW  Size (RW Data + ZI Data)             14104 (  13.77kB)
    Total ROM Size (Code + RO Data + RW Data)      51640 (  50.43kB)

==============================================================================

