Component: ARM Compiler 5.06 update 6 (build 750) Tool: armlink [4d35ed]

==============================================================================

Section Cross References

    main.o(i.main) refers to board.o(i.board_Init) for board_Init
    main.o(i.main) refers to s8_demo.o(i.s8_demo) for s8_demo
    main.o(i.main) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(i.app_tp_transfer_phone) for app_tp_transfer_phone
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(i.app_tp_s_write) for app_tp_s_write
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(.data) for i2cs_transfer
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(i.app_tp_phone_reset_init) for app_tp_phone_reset_init
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(i.app_tp_screen_int_init) for app_tp_screen_int_init
    app_tp_transfer.o(i.app_tp_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(i.screen_spim_io_init) for screen_spim_io_init
    app_tp_transfer.o(i.app_tp_init) refers to hal_spi_master.o(i.hal_spim_init) for hal_spim_init
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(i.phone_i2cs_io_init) for phone_i2cs_io_init
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_slave.o(i.hal_i2cs_init) for hal_i2cs_init
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_slave.o(i.hal_i2cs_register_callback) for hal_i2cs_register_callback
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) for hal_i2cs_update_rx_buffer
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer) for hal_i2cs_update_tx_buffer
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_slave.o(i.hal_i2cs_start) for hal_i2cs_start
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_for_custom_s8.o(.data) for g_phone_output_int_pad
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(i.app_tp_i2cs_callback) for app_tp_i2cs_callback
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(.bss) for s_phone_read_buffer
    app_tp_transfer.o(i.app_tp_m_read) refers to hal_spi_master.o(i.hal_spim_read) for hal_spim_read
    app_tp_transfer.o(i.app_tp_m_transfer_complate) refers to hal_spi_master.o(i.hal_spim_get_transfer_complete) for hal_spim_get_transfer_complete
    app_tp_transfer.o(i.app_tp_m_write) refers to hal_spi_master.o(i.hal_spim_write) for hal_spim_write
    app_tp_transfer.o(i.app_tp_m_write) refers to app_tp_transfer.o(.data) for s_spim_write
    app_tp_transfer.o(i.app_tp_phone_clear_reset_on) refers to app_tp_transfer.o(.data) for s_phone_reset_flag
    app_tp_transfer.o(i.app_tp_phone_reset_init) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    app_tp_transfer.o(i.app_tp_phone_reset_init) refers to hal_gpio.o(i.hal_gpio_ctrl_eint) for hal_gpio_ctrl_eint
    app_tp_transfer.o(i.app_tp_phone_reset_init) refers to hal_gpio.o(i.hal_gpio_init_eint) for hal_gpio_init_eint
    app_tp_transfer.o(i.app_tp_phone_reset_init) refers to hal_gpio.o(i.hal_gpio_reg_eint_cb) for hal_gpio_reg_eint_cb
    app_tp_transfer.o(i.app_tp_phone_reset_init) refers to app_tp_for_custom_s8.o(.data) for g_phone_input_rst_pad
    app_tp_transfer.o(i.app_tp_phone_reset_init) refers to app_tp_transfer.o(i.app_tp_reset_callback) for app_tp_reset_callback
    app_tp_transfer.o(i.app_tp_phone_reset_on) refers to app_tp_transfer.o(.data) for s_phone_reset_flag
    app_tp_transfer.o(i.app_tp_reset_callback) refers to app_tp_transfer.o(.data) for s_phone_reset_flag
    app_tp_transfer.o(i.app_tp_s_read) refers to hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) for hal_i2cs_update_rx_buffer
    app_tp_transfer.o(i.app_tp_s_write) refers to hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer) for hal_i2cs_update_tx_buffer
    app_tp_transfer.o(i.app_tp_screen_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    app_tp_transfer.o(i.app_tp_screen_init) refers to tau_delay.o(i.delayUs) for delayUs
    app_tp_transfer.o(i.app_tp_screen_init) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_transfer.o(i.app_tp_screen_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_rst_pad
    app_tp_transfer.o(i.app_tp_screen_int_callback) refers to app_tp_transfer.o(.data) for s_screen_int_flag
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to hal_gpio.o(i.hal_gpio_ctrl_eint) for hal_gpio_ctrl_eint
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to hal_gpio.o(i.hal_gpio_init_eint) for hal_gpio_init_eint
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to hal_gpio.o(i.hal_gpio_reg_eint_cb) for hal_gpio_reg_eint_cb
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to app_tp_transfer.o(i.app_tp_screen_int_callback) for app_tp_screen_int_callback
    app_tp_transfer.o(i.app_tp_screen_int_lvl_low) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    app_tp_transfer.o(i.app_tp_screen_int_lvl_low) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.app_tp_transfer_phone) refers to app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) for app_tp_phone_analysis_data
    app_tp_transfer.o(i.app_tp_transfer_phone) refers to app_tp_transfer.o(i.app_tp_s_read) for app_tp_s_read
    app_tp_transfer.o(i.app_tp_transfer_phone) refers to app_tp_transfer.o(.data) for s_slave_txbuffer_size
    app_tp_transfer.o(i.app_tp_transfer_phone) refers to app_tp_transfer.o(.bss) for s_phone_read_buffer
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(i.app_tp_m_transfer_complate) for app_tp_m_transfer_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to hal_spi_master.o(i.hal_spim_flush) for hal_spim_flush
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) for app_tp_screen_analysis_const
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(.data) for s_screen_const_transfer_count
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_for_custom_s8.o(.constdata) for screen_reg_start_data_size
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_for_custom_s8.o(.data) for screen_reg_start_data
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(.bss) for s_screen_read_buffer
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_transfer_screen_const) for app_tp_transfer_screen_const
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_screen_int_lvl_low) for app_tp_screen_int_lvl_low
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_m_transfer_complate) for app_tp_m_transfer_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_spi_master.o(i.hal_spim_flush) for hal_spim_flush
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) for app_tp_screen_analysis_int
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_system.o(i.hal_system_get_tick) for hal_system_get_tick
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(i.app_tp_write_other_operations) for app_tp_write_other_operations
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(.data) for s_screen_init_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(.data) for screen_reg_int_data
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(.bss) for s_screen_read_buffer
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(.constdata) for screen_reg_int_data_size
    app_tp_transfer.o(i.app_tp_transfer_screen_start) refers to app_tp_transfer.o(i.app_tp_screen_init) for app_tp_screen_init
    app_tp_transfer.o(i.app_tp_transfer_screen_start) refers to app_tp_transfer.o(i.app_tp_transfer_screen_const) for app_tp_transfer_screen_const
    app_tp_transfer.o(i.app_tp_transfer_screen_start) refers to app_tp_transfer.o(.data) for s_screen_init_complate
    app_tp_transfer.o(i.phone_i2cs_io_init) refers to hal_gpio.o(i.hal_gpio_config_pad) for hal_gpio_config_pad
    app_tp_transfer.o(i.phone_i2cs_io_init) refers to app_tp_transfer.o(.constdata) for .constdata
    app_tp_transfer.o(i.screen_spim_io_init) refers to hal_gpio.o(i.hal_gpio_config_pad) for hal_gpio_config_pad
    app_tp_transfer.o(i.screen_spim_io_init) refers to app_tp_transfer.o(.constdata) for .constdata
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to app_tp_for_custom_s8.o(.data) for start_now
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to app_tp_for_custom_s8.o(.constdata) for phone_60_start_back
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to app_tp_transfer.o(i.app_tp_screen_init) for app_tp_screen_init
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to app_tp_for_custom_s8.o(.data) for app_tp_count
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to ffltui.o(.text) for __aeabi_ui2f
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to fmul.o(.text) for __aeabi_fmul
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to fdiv.o(.text) for __aeabi_fdiv
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to ffixui.o(.text) for __aeabi_f2uiz
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to f2d.o(.text) for __aeabi_f2d
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to dmul.o(.text) for __aeabi_dmul
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to ddiv.o(.text) for __aeabi_ddiv
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to dfixui.o(.text) for __aeabi_d2uiz
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to app_tp_for_custom_s8.o(.data) for phone_reg_coord_BUF_NUM
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to app_tp_for_custom_s8.o(.bss) for Touch
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_for_custom_s8.o(i.app_tp_write_other_operations) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_for_custom_s8.o(i.app_tp_write_other_operations) refers to app_tp_for_custom_s8.o(.data) for start_now
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.constdata) for screen_87_data
    s8_demo.o(i.PhoneDisOffDeal) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    s8_demo.o(i.PhoneDisOffDeal) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    s8_demo.o(i.PhoneDisOffDeal) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    s8_demo.o(i.PhoneDisOffDeal) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    s8_demo.o(i.PhoneDisOffDeal) refers to hal_system.o(i.hal_system_get_tick) for hal_system_get_tick
    s8_demo.o(i.PhoneDisOffDeal) refers to s8_demo.o(.data) for Flag
    s8_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) for hal_dsi_rx_ctrl_send_ack_cmd
    s8_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) for hal_dsi_rx_ctrl_get_max_ret_size
    s8_demo.o(i.ap_dcs_read) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.ap_dcs_read) refers to s8_demo.o(.data) for g_rx_ctrl_handle
    s8_demo.o(i.ap_dcs_set_AOD_53) refers to s8_demo.o(.data) for sg_aod_in_flag
    s8_demo.o(i.ap_dcs_set_backlight) refers to idiv.o(.text) for __aeabi_idivmod
    s8_demo.o(i.ap_dcs_set_backlight) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    s8_demo.o(i.ap_dcs_set_backlight) refers to s8_demo.o(.data) for AP_REG51_7FF
    s8_demo.o(i.ap_dcs_set_display_on) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    s8_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to tau_delay.o(i.delayMs) for delayMs
    s8_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    s8_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    s8_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to s8_demo.o(i.ap_rstn_pull_down_cb) for ap_rstn_pull_down_cb
    s8_demo.o(i.ap_dcs_set_exit_sleep_mode) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    s8_demo.o(i.ap_dcs_set_exit_sleep_mode) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.ap_dcs_set_eye_protection_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) for hal_dsi_tx_ctrl_set_ccm
    s8_demo.o(i.ap_rstn_pull_down_cb) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    s8_demo.o(i.ap_rstn_pull_down_cb) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.ap_rstn_pull_down_cb) refers to s8_demo.o(.data) for sg_system_suspend
    s8_demo.o(i.ap_rstn_pull_high_cb) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    s8_demo.o(i.ap_rstn_pull_high_cb) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.ap_rstn_pull_high_cb) refers to s8_demo.o(.data) for sg_system_resume
    s8_demo.o(i.ap_set_framerate) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode) for hal_dsi_tx_ctrl_set_tear_mode
    s8_demo.o(i.ap_set_framerate) refers to s8_demo.o(.data) for g_tx_ctrl_handle
    s8_demo.o(i.ap_update_pps_9E) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) for hal_dsi_rx_ctrl_pre_init_pps
    s8_demo.o(i.ap_update_pps_9E) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) for hal_dsi_rx_ctrl_toggle_resolution
    s8_demo.o(i.ap_update_pps_9E) refers to s8_demo.o(.data) for g_rx_ctrl_handle
    s8_demo.o(i.app_display_init) refers to s8_demo.o(i.app_mipi_rx_init) for app_mipi_rx_init
    s8_demo.o(i.app_display_init) refers to hal_pwr.o(i.hal_pwr_get_vcc_power_ready) for hal_pwr_get_vcc_power_ready
    s8_demo.o(i.app_display_init) refers to s8_demo.o(i.app_gpio_init) for app_gpio_init
    s8_demo.o(i.app_display_init) refers to hal_swire.o(i.hal_swire_init) for hal_swire_init
    s8_demo.o(i.app_display_init) refers to hal_swire.o(i.hal_swire_set_timer) for hal_swire_set_timer
    s8_demo.o(i.app_display_init) refers to s8_demo.o(i.app_mipi_tx_init) for app_mipi_tx_init
    s8_demo.o(i.app_display_init) refers to s8_demo.o(i.app_mipi_tx_start) for app_mipi_tx_start
    s8_demo.o(i.app_gpio_init) refers to memcpya.o(.text) for __aeabi_memcpy4
    s8_demo.o(i.app_gpio_init) refers to hal_gpio.o(i.hal_gpio_config_pad) for hal_gpio_config_pad
    s8_demo.o(i.app_gpio_init) refers to s8_demo.o(.constdata) for .constdata
    s8_demo.o(i.app_init_panel) refers to s8_demo.o(i.app_tx_panel_reset) for app_tx_panel_reset
    s8_demo.o(i.app_init_panel) refers to s8_demo.o(i.send_panel_init_code) for send_panel_init_code
    s8_demo.o(i.app_init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    s8_demo.o(i.app_init_panel) refers to tau_delay.o(i.delayMs) for delayMs
    s8_demo.o(i.app_init_panel) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    s8_demo.o(i.app_init_panel) refers to hal_swire.o(i.hal_swire_enable) for hal_swire_enable
    s8_demo.o(i.app_init_panel) refers to hal_swire.o(i.hal_swire_set_pulse) for hal_swire_set_pulse
    s8_demo.o(i.app_init_panel) refers to s8_demo.o(.constdata) for panel_init_code
    s8_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) for hal_dsi_rx_ctrl_create_handle
    s8_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) for hal_dsi_rx_ctrl_pre_init_pps
    s8_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    s8_demo.o(i.app_mipi_rx_init) refers to s8_demo.o(i.app_set_dcs_hw_ack) for app_set_dcs_hw_ack
    s8_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    s8_demo.o(i.app_mipi_rx_init) refers to s8_demo.o(.data) for g_rx_ctrl_handle
    s8_demo.o(i.app_mipi_rx_init) refers to s8_demo.o(.constdata) for g_cus_rx_dcs_execute_table
    s8_demo.o(i.app_mipi_rx_init) refers to s8_demo.o(i.pps_update_handle) for pps_update_handle
    s8_demo.o(i.app_mipi_rx_start_cb) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    s8_demo.o(i.app_mipi_rx_start_cb) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    s8_demo.o(i.app_mipi_rx_start_cb) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.app_mipi_rx_start_cb) refers to s8_demo.o(.data) for g_rx_ctrl_handle
    s8_demo.o(i.app_mipi_tx_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) for hal_dsi_tx_ctrl_create_handle
    s8_demo.o(i.app_mipi_tx_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    s8_demo.o(i.app_mipi_tx_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) for hal_dsi_tx_ctrl_set_overwrite_rgb
    s8_demo.o(i.app_mipi_tx_init) refers to s8_demo.o(.data) for g_tx_ctrl_handle
    s8_demo.o(i.app_mipi_tx_start) refers to s8_demo.o(i.app_init_panel) for app_init_panel
    s8_demo.o(i.app_mipi_tx_start) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    s8_demo.o(i.app_mipi_tx_start) refers to tau_delay.o(i.delayMs) for delayMs
    s8_demo.o(i.app_mipi_tx_start) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    s8_demo.o(i.app_mipi_tx_start) refers to hal_swire.o(i.hal_swire_set_pulse) for hal_swire_set_pulse
    s8_demo.o(i.app_mipi_tx_start) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.app_mipi_tx_start) refers to s8_demo.o(.data) for g_tx_ctrl_handle
    s8_demo.o(i.app_set_dcs_hw_ack) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack) for hal_dsi_rx_ctrl_set_auto_ack
    s8_demo.o(i.app_set_dcs_hw_ack) refers to s8_demo.o(.data) for g_rx_ctrl_handle
    s8_demo.o(i.app_system_process) refers to s8_demo.o(i.app_system_suspend) for app_system_suspend
    s8_demo.o(i.app_system_process) refers to s8_demo.o(i.app_system_resume) for app_system_resume
    s8_demo.o(i.app_system_process) refers to s8_demo.o(.data) for sg_system_suspend
    s8_demo.o(i.app_system_resume) refers to hal_pwr.o(i.hal_pwr_exit_sleep_mode) for hal_pwr_exit_sleep_mode
    s8_demo.o(i.app_system_resume) refers to s8_demo.o(i.app_display_init) for app_display_init
    s8_demo.o(i.app_system_resume) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.app_system_suspend) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) for hal_dsi_tx_ctrl_stop
    s8_demo.o(i.app_system_suspend) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) for hal_dsi_tx_ctrl_deinit
    s8_demo.o(i.app_system_suspend) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) for hal_dsi_rx_ctrl_stop
    s8_demo.o(i.app_system_suspend) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) for hal_dsi_rx_ctrl_deinit
    s8_demo.o(i.app_system_suspend) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    s8_demo.o(i.app_system_suspend) refers to hal_swire.o(i.hal_swire_deinit) for hal_swire_deinit
    s8_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_set_sleep_mode_power) for hal_pwr_set_sleep_mode_power
    s8_demo.o(i.app_system_suspend) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    s8_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_set_pvd) for hal_pwr_set_pvd
    s8_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_enter_normal_sleep_mode) for hal_pwr_enter_normal_sleep_mode
    s8_demo.o(i.app_system_suspend) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) for hal_pwr_set_stop_sleep_wakeup_pin
    s8_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) for hal_pwr_enter_stop_sleep_mode
    s8_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode) for hal_pwr_enter_deep_sleep_mode
    s8_demo.o(i.app_system_suspend) refers to s8_demo.o(.data) for g_tx_ctrl_handle
    s8_demo.o(i.app_system_suspend) refers to s8_demo.o(i.ap_rstn_pull_high_cb) for ap_rstn_pull_high_cb
    s8_demo.o(i.app_tx_panel_reset) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    s8_demo.o(i.app_tx_panel_reset) refers to tau_delay.o(i.delayMs) for delayMs
    s8_demo.o(i.pps_update_handle) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) for hal_dsi_rx_ctrl_toggle_resolution
    s8_demo.o(i.pps_update_handle) refers to s8_demo.o(.data) for g_rx_ctrl_handle
    s8_demo.o(i.s8_demo) refers to hal_pwr.o(i.hal_pwr_set_main_power) for hal_pwr_set_main_power
    s8_demo.o(i.s8_demo) refers to s8_demo.o(i.app_display_init) for app_display_init
    s8_demo.o(i.s8_demo) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.s8_demo) refers to s8_demo.o(i.PhoneDisOffDeal) for PhoneDisOffDeal
    s8_demo.o(i.s8_demo) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) for hal_dsi_rx_ctrl_dcs_async_handler
    s8_demo.o(i.s8_demo) refers to s8_demo.o(i.app_system_process) for app_system_process
    s8_demo.o(i.s8_demo) refers to s8_demo.o(.data) for g_rx_ctrl_handle
    s8_demo.o(i.send_panel_init_code) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) for hal_dsi_tx_ctrl_write_array_cmd
    s8_demo.o(i.send_panel_init_code) refers to tau_delay.o(i.delayUs) for delayUs
    s8_demo.o(i.soft_swire_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    s8_demo.o(i.soft_swire_init) refers to tau_delay.o(i.delayMs) for delayMs
    s8_demo.o(i.soft_swire_init) refers to s8_demo.o(i.soft_swire_start) for soft_swire_start
    s8_demo.o(i.soft_swire_init) refers to hal_timer.o(i.hal_timer_init) for hal_timer_init
    s8_demo.o(i.soft_swire_init) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    s8_demo.o(i.soft_swire_init) refers to s8_demo.o(.data) for s_swire_pwm_counter
    s8_demo.o(i.soft_swire_init) refers to s8_demo.o(i.soft_swire_timer_callback) for soft_swire_timer_callback
    s8_demo.o(i.soft_swire_start) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    s8_demo.o(i.soft_swire_start) refers to tau_delay.o(i.delayUs) for delayUs
    s8_demo.o(i.soft_swire_timer_callback) refers to s8_demo.o(i.soft_swire_start) for soft_swire_start
    s8_demo.o(i.soft_swire_timer_callback) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    s8_demo.o(i.soft_swire_timer_callback) refers to hal_timer.o(i.hal_timer_deinit) for hal_timer_deinit
    s8_demo.o(i.soft_swire_timer_callback) refers to hal_timer.o(i.hal_timer_stop) for hal_timer_stop
    s8_demo.o(i.soft_swire_timer_callback) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    s8_demo.o(i.soft_swire_timer_callback) refers to s8_demo.o(.data) for s_swire_pwm_counter
    s8_demo.o(.constdata) refers to s8_demo.o(i.ap_dcs_set_display_on) for ap_dcs_set_display_on
    s8_demo.o(.constdata) refers to s8_demo.o(i.ap_dcs_set_display_off) for ap_dcs_set_display_off
    s8_demo.o(.constdata) refers to s8_demo.o(i.ap_dcs_set_backlight) for ap_dcs_set_backlight
    s8_demo.o(.constdata) refers to s8_demo.o(i.ap_dcs_set_AOD_53) for ap_dcs_set_AOD_53
    s8_demo.o(.constdata) refers to s8_demo.o(i.ap_dcs_set_enter_sleep_mode) for ap_dcs_set_enter_sleep_mode
    s8_demo.o(.constdata) refers to s8_demo.o(i.ap_dcs_set_exit_sleep_mode) for ap_dcs_set_exit_sleep_mode
    s8_demo.o(.constdata) refers to s8_demo.o(i.ap_update_pps_9E) for ap_update_pps_9E
    s8_demo.o(.constdata) refers to s8_demo.o(i.ap_set_framerate) for ap_set_framerate
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_init) for hal_system_init
    board.o(i.board_Init) refers to tau_log.o(i.tau_log_init) for tau_log_init
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_enable_systick) for hal_system_enable_systick
    startup_armcm0.o(RESET) refers to startup_armcm0.o(STACK) for __initial_sp
    startup_armcm0.o(RESET) refers to startup_armcm0.o(.text) for Reset_Handler
    startup_armcm0.o(RESET) refers to drv_common.o(i.HardFault_Handler) for HardFault_Handler
    startup_armcm0.o(RESET) refers to drv_common.o(i.SysTick_Handler) for SysTick_Handler
    startup_armcm0.o(RESET) refers to drv_vidc.o(i.VIDC_IRQn_Handler) for VIDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to hal_internal_vsync.o(i.LCDC_IRQn_Handler) for LCDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) for MIPI_RX_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler) for MIPI_TX_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_memc.o(i.MEMC_IRQn_Handler) for MEMC_IRQn_Handler
    startup_armcm0.o(RESET) refers to hal_internal_dcs.o(i.VPRE_IRQn_Handler) for VPRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_dma.o(i.DMA_IRQn_Handler) for DMA_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER0_IRQn_Handler) for TIMER0_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER1_IRQn_Handler) for TIMER1_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER2_IRQn_Handler) for TIMER2_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER3_IRQn_Handler) for TIMER3_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_uart.o(i.UART_IRQn_Handler) for UART_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_i2c.o(i.I2C0_IRQn_Handler) for I2C0_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_i2c.o(i.I2C1_IRQn_Handler) for I2C1_IRQn_Handler
    startup_armcm0.o(RESET) refers to hal_spi_master.o(i.SPIM_IRQn_Handler) for SPIM_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_rxbr.o(i.VPRE1_IRQn_Handler) for VPRE1_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_i2c.o(i.I2C2_IRQn_Handler) for I2C2_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_swire.o(i.SWIRE_IRQn_Handler) for SWIRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.AP_NRESET_IRQn_Handler) for AP_NRESET_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT0_IRQn_Handler) for EXTI_INT0_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT1_IRQn_Handler) for EXTI_INT1_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT2_IRQn_Handler) for EXTI_INT2_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT3_IRQn_Handler) for EXTI_INT3_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT4_IRQn_Handler) for EXTI_INT4_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT5_IRQn_Handler) for EXTI_INT5_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT6_IRQn_Handler) for EXTI_INT6_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT7_IRQn_Handler) for EXTI_INT7_IRQn_Handler
    startup_armcm0.o(.text) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd) refers to drv_rxbr.o(i.drv_rxbr_set_ack_pkt_md) for drv_rxbr_set_ack_pkt_md
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_lpdt_fifo_status) for drv_dsi_rx_get_lpdt_fifo_status
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) for dcs_packet_get_fifo_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) for dcs_packet_free_fifo_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) for hal_internal_vsync_get_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_reset_modules) for drv_crgu_reset_modules
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_rxbr.o(i.drv_rxbr_swpxl_clr) for drv_rxbr_swpxl_clr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_rxbr.o(i.drv_rxbr_set_cmd_filter) for drv_rxbr_set_cmd_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_vidc.o(i.drv_vidc_set_src_parameter) for drv_vidc_set_src_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_vidc.o(i.drv_vidc_set_pu_ctrl) for drv_vidc_set_pu_ctrl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_rxbr.o(i.drv_rxbr_set_swpxl_data) for drv_rxbr_set_swpxl_data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg) for drv_dsi_rx_set_ddi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) for hal_dsi_rx_ctrl_set_rx_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg) for drv_dsi_rx_set_ipi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.constdata) for .constdata
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_force_video_crtl) refers to drv_dsi_rx.o(i.drv_dsi_rx_force_video_crtl) for drv_dsi_rx_force_video_crtl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size) for drv_dsi_rx_get_max_ret_size
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) for hal_dsi_rx_ctrl_init_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_rx) for hal_internal_vsync_init_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) for hal_dsi_rx_ctrl_init_dsi_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) for hal_dsi_rx_ctrl_init_rxbr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_irqen) for drv_dsc_dec_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) for hal_dsi_rx_ctrl_init_vidc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) for hal_dsi_rx_ctrl_init_memc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_se.o(i.drv_se_start_rx) for drv_se_start_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_pwr.o(i.drv_pwr_set_pll_clk) for drv_pwr_set_pll_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_clk) for drv_crgu_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dsc_clk) for drv_crgu_set_dsc_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_vidc_clk) for drv_crgu_set_vidc_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_fb_clk) for drv_crgu_set_fb_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg) for drv_dsi_rx_set_ctrl_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) for drv_dsi_rx_set_up_phy
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap) for drv_dsi_rx_set_lane_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_crc_en) for drv_dsi_rx_set_ddi_crc_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_ycbcr_frmt) for drv_dsi_rx_set_ipi_ycbcr_frmt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_tear_resp_en) for drv_dsi_rx_set_tear_resp_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_inten) for drv_dsi_rx_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc) for drv_dsi_rx_set_check_crc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt) for drv_dsi_rx_set_resp_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_mode) for drv_memc_set_ltpo_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_fs_en_conditions) for drv_memc_set_fs_en_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_lcdc_st_conditions) for drv_memc_set_lcdc_st_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_vidc_sync_cnt) for drv_memc_set_vidc_sync_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_double_buffer) for drv_memc_set_double_buffer
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_circ_mode_enable) for drv_memc_set_circ_mode_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_active_height) for drv_memc_set_active_height
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_pu_thres) for drv_memc_set_ltpo_pu_thres
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_color_format) for drv_rxbr_set_color_format
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th) for drv_rxbr_set_ltpo_drop_th
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_cfg) for drv_rxbr_set_usr_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_col) for drv_rxbr_set_usr_col
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_row) for drv_rxbr_set_usr_row
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg) for drv_rxbr_hline_rcv_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) for hal_intl_dcs_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_src_parameter) for drv_vidc_set_src_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pentile_swap) for drv_vidc_set_pentile_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_dst_parameter) for drv_vidc_set_dst_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_circ_mode_enable) for drv_vidc_set_circ_mode_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_init_module_enable) for drv_vidc_init_module_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_dither_config) for drv_vidc_set_dither_config
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_vintp_config) for drv_vidc_set_vintp_config
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_rotation) for drv_vidc_set_rotation
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef0) for drv_vidc_set_scld_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef1) for drv_vidc_set_scld_hcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef0) for drv_vidc_set_scld_vcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef1) for drv_vidc_set_scld_vcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_honly_hinitr) for drv_vidc_set_honly_hinitr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_honly_hinitb) for drv_vidc_set_honly_hinitb
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_honly_hcoef0) for drv_vidc_set_honly_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_mirror) for drv_vidc_set_mirror
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pu_ctrl) for drv_vidc_set_pu_ctrl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_dsi_rx_ctrl.o(.constdata) for .constdata
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to hal_internal_vsync.o(i.hal_internal_sync_register_rx_callback) for hal_internal_sync_register_rx_callback
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to drv_vidc.o(i.drv_vidc_set_irq_line) for drv_vidc_set_irq_line
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_write_cmd_entry) refers to hal_internal_dcs.o(i.hal_intl_dcs_register_write_cmd_entry) for hal_intl_dcs_register_write_cmd_entry
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header) for drv_rxbr_set_ack_pkt_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack) refers to drv_rxbr.o(i.drv_rxbr_set_cmd_response) for drv_rxbr_set_cmd_response
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) for hal_intl_dcs_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_check_crc) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc) for drv_dsi_rx_set_check_crc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_check_crc) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) for drv_dsi_rx_calc_ipi_tx_delay
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg) for drv_dsi_rx_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_log_level) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_drv_log_level) for drv_dsi_rx_set_drv_log_level
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to drv_rxbr.o(i.drv_rxbr_sw_reset) for drv_rxbr_sw_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) for hal_dsi_rx_ctrl_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) for hal_intl_svs_update_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_clk) for drv_crgu_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_dsi_rx.o(i.drv_dsi_rx_power_up) for drv_dsi_rx_power_up
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) for hal_internal_vsync_toggle_input_frame_rate
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) for hal_internal_sync_input_resolution_change
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) for hal_dsi_tx_ctrl_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg) for drv_dsi_tx_phy_time_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) for drv_dsi_tx_phy_test_setup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready) for drv_dsi_tx_phy_status_ready
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_crgu.o(i.drv_crgu_reset_modules) for drv_crgu_reset_modules
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_reset_modules) for drv_crgu_reset_modules
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb) for hal_internal_sync_register_lcdc_cb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) for hal_internal_sync_set_fb_setting_manual
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) for hal_lcdc_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_frame) refers to drv_lcdc.o(i.drv_lcdc_fixed_frame_output) for drv_lcdc_fixed_frame_output
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_get_tear_mode) for drv_memc_get_tear_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_gen_a_tear_signal) for drv_memc_gen_a_tear_signal
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_tx) for hal_internal_vsync_init_tx
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb) for hal_internal_sync_register_lcdc_cb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) for hal_dsi_tx_ctrl_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) for hal_dsi_tx_init_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) for hal_dsi_tx_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) for hal_lcdc_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) for hal_lcdc_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready) for drv_dsi_tx_phy_status_ready
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) for hal_nonshadow_func_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_vsync_func_update) for hal_vsync_func_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_overwrite_enable) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_overwrite_enable) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_partial_disp_enable) refers to drv_lcdc.o(i.drv_lcdc_part_display_config) for drv_lcdc_part_display_config
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_partial_disp_enable) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload) for drv_dsi_tx_command_get_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) for hal_nonshadow_func_req_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_sync_line) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) for hal_internal_vsync_set_sync_line
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_sync_line) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) for hal_nonshadow_func_req_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) for hal_nonshadow_func_req_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) for hal_nonshadow_func_req_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb) for drv_lcdc_config_overwrite_rgb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_vpg) for drv_dsi_tx_set_vpg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) for hal_dsi_tx_ctrl_draw_flick
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp) for drv_dsi_tx_phy_clock_lane_auto_lp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_cfg_int_frame) for drv_lcdc_cfg_int_frame
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_enable_shadow_reg) for drv_lcdc_enable_shadow_reg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_start) for hal_lcdc_start
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_lcdc.o(i.drv_lcdc_stop_display) for drv_lcdc_stop_display
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) for hal_dsi_tx_ctrl_read_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg) for drv_dsi_tx_video_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack) for drv_dsi_tx_set_bta_ack
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time) for drv_dsi_tx_dpi_lpcmd_time
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode) for drv_dsi_tx_phy_lane_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode) for drv_dsi_tx_dpi_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity) for drv_dsi_tx_dpi_polarity
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_response_mode) for drv_dsi_tx_response_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div) for drv_dsi_tx_set_time_out_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg) for drv_dsi_tx_timeout_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp) for drv_dsi_tx_phy_clock_lane_auto_lp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_int) for drv_dsi_tx_config_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to drv_crgu.o(i.drv_crgu_set_dpi_clk) for drv_crgu_set_dpi_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to hal_dsi_tx_ctrl.o(.constdata) for .constdata
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg) for drv_dsi_tx_phy_time_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) for drv_dsi_tx_phy_test_setup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update) for hal_dsi_tx_timing_info_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) for hal_dsi_tx_cmd_mode_cal_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size) for drv_dsi_tx_edpi_cmd_size
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) for hal_dsi_tx_init_phy_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) for hal_dsi_tx_init_dpi_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) for hal_dsi_tx_vid_mode_cal_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing) for hal_dsi_tx_init_vid_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk) for drv_dsi_tx_set_video_chunk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing) for drv_dsi_tx_set_video_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_header) for drv_dsi_tx_command_header
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update) refers to d2f.o(.text) for __aeabi_d2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_internal_svs.o(i.hal_intl_svs_init_tx) for hal_intl_svs_init_tx
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) for hal_tx_frame_rate_adjust
    hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) refers to drv_lcdc.o(i.drv_lcdc_endianness_config) for drv_lcdc_endianness_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) refers to drv_lcdc.o(i.drv_lcdc_crop_hact) for drv_lcdc_crop_hact
    hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) for hal_lcdc_postproc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) for hal_lcdc_displayproc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) for hal_intl_fb_get_tx_fb_info
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) for hal_lcdc_timinggen_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to drv_lcdc.o(i.drv_lcdc_config_int) for drv_lcdc_config_int
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fscalb.o(.text) for __ARM_scalbnf
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_lcdc_clk) for drv_crgu_set_lcdc_clk
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) for hal_intl_fb_get_tx_fb_info
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) for hal_lcdc_upscaler_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_fldc_config) for drv_lcdc_fldc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_bcsa_config) for drv_lcdc_bcsa_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_fc_config) for drv_lcdc_fc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_edge_dect_config) for drv_lcdc_edge_dect_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_edge_enh_config) for drv_lcdc_edge_enh_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_vintp_mode_config) for drv_lcdc_vintp_mode_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_dith_config) for drv_lcdc_dith_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to drv_lcdc.o(i.drv_lcdc_vid_hw_start) for drv_lcdc_vid_hw_start
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to drv_lcdc.o(i.drv_lcdc_cmd_start) for drv_lcdc_cmd_start
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to drv_lcdc.o(i.drv_lcdc_ctrl_flow) for drv_lcdc_ctrl_flow
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to drv_lcdc.o(i.drv_lcdc_config_src_parameter) for drv_lcdc_config_src_parameter
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to drv_lcdc.o(i.drv_lcdc_set_prefetch) for drv_lcdc_set_prefetch
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for sg_pq_para
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_bcsa_config) for drv_lcdc_bcsa_config
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_fc_config) for drv_lcdc_fc_config
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_edge_dect_config) for drv_lcdc_edge_dect_config
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_edge_enh_config) for drv_lcdc_edge_enh_config
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for sg_pq_para
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to cfcmple.o(.text) for __aeabi_cfcmple
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_vsync_func_update) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_vsync_func_update) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_gpio.o(i.hal_gpio_config_pad) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_config_pad) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    hal_gpio.o(i.hal_gpio_config_pad) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    hal_gpio.o(i.hal_gpio_ctrl_eint) refers to drv_gpio.o(i.drv_gpio_set_int) for drv_gpio_set_int
    hal_gpio.o(i.hal_gpio_get_input_data) refers to drv_gpio.o(i.drv_gpio_get_input_data) for drv_gpio_get_input_data
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_eint) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group) for drv_sys_cfg_sel_gpio_group
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig) for drv_sys_cfg_sel_int_trig
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_init_input) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_input) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_init_output) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_reg_eint_cb) refers to drv_gpio.o(i.drv_gpio_register_callback) for drv_gpio_register_callback
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_gpio.o(i.drv_gpio_register_ap_reset_callback) for drv_gpio_register_ap_reset_callback
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) for drv_sys_cfg_sel_ap_rst_trig
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_high_impedance) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode) for drv_gpio_set_mode
    hal_gpio.o(i.hal_gpio_set_mode) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_output_data) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to hal_gpio.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_i2c.o(i.drv_i2c_get_intr_status) for drv_i2c_get_intr_status
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_i2c.o(i.drv_i2c_get_rx_count) for drv_i2c_get_rx_count
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_i2c.o(i.drv_i2c_flush) for drv_i2c_flush
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_i2c.o(i.drv_i2c_clear_intr_status) for drv_i2c_clear_intr_status
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_dma.o(i.drv_dma_get_remaining_trans_num) for drv_dma_get_remaining_trans_num
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_dma.o(i.drv_dma_set_mem_trans_offset) for drv_dma_set_mem_trans_offset
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_dma.o(i.drv_dma_enable) for drv_dma_enable
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_i2c.o(i.drv_i2c_get_fifo_status) for drv_i2c_get_fifo_status
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_i2c.o(i.drv_i2c_get_tx_abrtsource) for drv_i2c_get_tx_abrtsource
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_i2c.o(i.drv_i2c_write_data) for drv_i2c_write_data
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_deinit) refers to drv_dma.o(i.drv_dma_deinit) for drv_dma_deinit
    hal_i2c_slave.o(i.hal_i2cs_deinit) refers to drv_i2c.o(i.drv_i2c_clock_enable) for drv_i2c_clock_enable
    hal_i2c_slave.o(i.hal_i2cs_deinit) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_get_rx_cnt) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_get_tx_cnt) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_get_write_complete) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_init) refers to drv_i2c.o(i.drv_i2c_clock_enable) for drv_i2c_clock_enable
    hal_i2c_slave.o(i.hal_i2cs_init) refers to drv_i2c.o(i.drv_i2cs_init) for drv_i2cs_init
    hal_i2c_slave.o(i.hal_i2cs_init) refers to drv_i2c.o(i.drv_i2c_set_callback) for drv_i2c_set_callback
    hal_i2c_slave.o(i.hal_i2cs_init) refers to drv_dma.o(i.drv_dma_apply_handle) for drv_dma_apply_handle
    hal_i2c_slave.o(i.hal_i2cs_init) refers to drv_dma.o(i.drv_dma_set_bitwide) for drv_dma_set_bitwide
    hal_i2c_slave.o(i.hal_i2cs_init) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    hal_i2c_slave.o(i.hal_i2cs_init) refers to hal_i2c_slave.o(i.hal_i2cs_callback) for hal_i2cs_callback
    hal_i2c_slave.o(i.hal_i2cs_init) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_register_callback) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_rx_cnt_clear) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_set_continue_transfer) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_start) refers to drv_i2c.o(i.drv_i2c_enable_intr) for drv_i2c_enable_intr
    hal_i2c_slave.o(i.hal_i2cs_start) refers to drv_i2c.o(i.drv_i2c_enable) for drv_i2c_enable
    hal_i2c_slave.o(i.hal_i2cs_start) refers to drv_i2c.o(i.drv_i2c_enable_dma_req) for drv_i2c_enable_dma_req
    hal_i2c_slave.o(i.hal_i2cs_start) refers to drv_dma.o(i.drv_dma_register_callback) for drv_dma_register_callback
    hal_i2c_slave.o(i.hal_i2cs_start) refers to drv_dma.o(i.drv_dma_enable_int) for drv_dma_enable_int
    hal_i2c_slave.o(i.hal_i2cs_start) refers to drv_dma.o(i.drv_dma_enable) for drv_dma_enable
    hal_i2c_slave.o(i.hal_i2cs_start) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_start) refers to hal_i2c_slave.o(i.hal_i2cs_tx_dma_callback) for hal_i2cs_tx_dma_callback
    hal_i2c_slave.o(i.hal_i2cs_stop) refers to drv_i2c.o(i.drv_i2c_enable) for drv_i2c_enable
    hal_i2c_slave.o(i.hal_i2cs_stop) refers to drv_i2c.o(i.drv_i2c_disable_intr) for drv_i2c_disable_intr
    hal_i2c_slave.o(i.hal_i2cs_stop) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_i2c_slave.o(i.hal_i2cs_stop) refers to drv_i2c.o(i.drv_i2c_disable_dma_req) for drv_i2c_disable_dma_req
    hal_i2c_slave.o(i.hal_i2cs_stop) refers to drv_i2c.o(i.drv_i2c_flush) for drv_i2c_flush
    hal_i2c_slave.o(i.hal_i2cs_stop) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_tx_dma_callback) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) refers to drv_i2c.o(i.drv_i2c_disable_dma_req) for drv_i2c_disable_dma_req
    hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) refers to drv_i2c.o(i.drv_i2c_flush) for drv_i2c_flush
    hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) refers to drv_dma.o(i.drv_dma_set_mem_trans_info) for drv_dma_set_mem_trans_info
    hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) refers to drv_dma.o(i.drv_dma_enable) for drv_dma_enable
    hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) refers to drv_i2c.o(i.drv_i2c_enable_dma_req) for drv_i2c_enable_dma_req
    hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer) refers to drv_i2c.o(i.drv_i2c_disable_dma_req) for drv_i2c_disable_dma_req
    hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer) refers to drv_i2c.o(i.drv_i2c_flush) for drv_i2c_flush
    hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer) refers to drv_dma.o(i.drv_dma_set_mem_trans_info) for drv_dma_set_mem_trans_info
    hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer) refers to drv_dma.o(i.drv_dma_set_circle_mode) for drv_dma_set_circle_mode
    hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer) refers to drv_i2c.o(i.drv_i2c_enable_dma_req) for drv_i2c_enable_dma_req
    hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer) refers to hal_i2c_slave.o(.data) for .data
    hal_spi_master.o(i.SPIM_IRQn_Handler) refers to drv_spi_master.o(i.drv_spim_disable_int) for drv_spim_disable_int
    hal_spi_master.o(i.SPIM_IRQn_Handler) refers to drv_spi_master.o(i.drv_spim_set_inten) for drv_spim_set_inten
    hal_spi_master.o(i.SPIM_IRQn_Handler) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    hal_spi_master.o(i.SPIM_IRQn_Handler) refers to drv_spi_master.o(i.drv_spim_clear_int_status) for drv_spim_clear_int_status
    hal_spi_master.o(i.SPIM_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_spi_master.o(i.SPIM_IRQn_Handler) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spim_deinit) refers to drv_per_common.o(i.drv_per_set_clock) for drv_per_set_clock
    hal_spi_master.o(i.hal_spim_deinit) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spim_get_transfer_complete) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spim_init) refers to drv_per_common.o(i.drv_per_set_clock) for drv_per_set_clock
    hal_spi_master.o(i.hal_spim_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    hal_spi_master.o(i.hal_spim_init) refers to drv_spi_master.o(i.drv_spim_init) for drv_spim_init
    hal_spi_master.o(i.hal_spim_read) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    hal_spi_master.o(i.hal_spim_read) refers to drv_spi_master.o(i.drv_spim_read) for drv_spim_read
    hal_spi_master.o(i.hal_spim_read) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spim_write) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    hal_spi_master.o(i.hal_spim_write) refers to drv_spi_master.o(i.drv_spim_write) for drv_spim_write
    hal_spi_master.o(i.hal_spim_write) refers to hal_spi_master.o(.data) for .data
    hal_swire.o(i.hal_swire_deinit) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    hal_swire.o(i.hal_swire_deinit) refers to drv_swire.o(i.drv_swire_enable) for drv_swire_enable
    hal_swire.o(i.hal_swire_deinit) refers to drv_swire.o(i.drv_swire_register_callback) for drv_swire_register_callback
    hal_swire.o(i.hal_swire_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_swire.o(i.hal_swire_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_swire.o(i.hal_swire_deinit) refers to hal_timer.o(i.hal_timer_deinit) for hal_timer_deinit
    hal_swire.o(i.hal_swire_deinit) refers to hal_swire.o(.data) for .data
    hal_swire.o(i.hal_swire_enable) refers to drv_swire.o(i.drv_swire_set_power_down) for drv_swire_set_power_down
    hal_swire.o(i.hal_swire_enable) refers to drv_swire.o(i.drv_swire_get_pulse_count) for drv_swire_get_pulse_count
    hal_swire.o(i.hal_swire_enable) refers to drv_swire.o(i.drv_swire_set_trig_mode) for drv_swire_set_trig_mode
    hal_swire.o(i.hal_swire_enable) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_swire.o(i.hal_swire_enable) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    hal_swire.o(i.hal_swire_enable) refers to hal_swire.o(.data) for .data
    hal_swire.o(i.hal_swire_init) refers to drv_crgu.o(i.drv_crgu_set_clock_div) for drv_crgu_set_clock_div
    hal_swire.o(i.hal_swire_init) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_swire.o(i.hal_swire_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_swire.o(i.hal_swire_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_swire.o(i.hal_swire_init) refers to drv_swire.o(i.drv_swire_set_bit_time) for drv_swire_set_bit_time
    hal_swire.o(i.hal_swire_init) refers to drv_swire.o(i.drv_swire_set_power_down) for drv_swire_set_power_down
    hal_swire.o(i.hal_swire_init) refers to drv_swire.o(i.drv_swire_enable) for drv_swire_enable
    hal_swire.o(i.hal_swire_init) refers to drv_common.o(.data) for g_system_clock
    hal_swire.o(i.hal_swire_register_callback) refers to drv_swire.o(i.drv_swire_register_callback) for drv_swire_register_callback
    hal_swire.o(i.hal_swire_register_callback) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    hal_swire.o(i.hal_swire_set_pulse) refers to drv_swire.o(i.drv_swire_set_trig_mode) for drv_swire_set_trig_mode
    hal_swire.o(i.hal_swire_set_pulse) refers to drv_swire.o(i.drv_swire_set_pulse_count) for drv_swire_set_pulse_count
    hal_swire.o(i.hal_swire_set_pulse) refers to hal_swire.o(.data) for .data
    hal_swire.o(i.hal_swire_set_timer) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_swire_timer) for drv_sys_cfg_sel_swire_timer
    hal_swire.o(i.hal_swire_set_timer) refers to hal_timer.o(i.hal_timer_init) for hal_timer_init
    hal_swire.o(i.hal_swire_set_timer) refers to hal_timer.o(i.hal_timer_set_repeat) for hal_timer_set_repeat
    hal_swire.o(i.hal_swire_set_timer) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_swire.o(i.hal_swire_set_timer) refers to drv_swire.o(i.drv_swire_set_trig_mode) for drv_swire_set_trig_mode
    hal_swire.o(i.hal_swire_set_timer) refers to hal_swire.o(.data) for .data
    hal_swire.o(i.hal_swire_set_waveform) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_swire.o(i.hal_swire_set_waveform) refers to drv_swire.o(i.drv_swire_set_bit_time) for drv_swire_set_bit_time
    hal_swire.o(i.hal_swire_set_waveform) refers to drv_common.o(.data) for g_system_clock
    hal_system.o(i.hal_system_disable_systick) refers to drv_common.o(i.drv_common_disable_systick) for drv_common_disable_systick
    hal_system.o(i.hal_system_enable_systick) refers to drv_common.o(i.drv_common_enable_systick) for drv_common_enable_systick
    hal_system.o(i.hal_system_get_tick) refers to drv_common.o(i.drv_common_get_tick) for drv_common_get_tick
    hal_system.o(i.hal_system_idle_mode) refers to drv_common.o(i.drv_common_idle_mode) for drv_common_idle_mode
    hal_system.o(i.hal_system_init) refers to drv_pwr.o(i.drv_pwr_set_pll_clk) for drv_pwr_set_pll_clk
    hal_system.o(i.hal_system_init) refers to hal_system.o(i.hal_system_updata_sysclk) for hal_system_updata_sysclk
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_system.o(i.hal_system_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int) for drv_sys_cfg_clear_all_int
    hal_system.o(i.hal_system_init) refers to drv_common.o(i.drv_common_system_init) for drv_common_system_init
    hal_system.o(i.hal_system_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_system.o(i.hal_system_register_systick_cb) refers to drv_common.o(i.drv_common_systick_register_cb) for drv_common_systick_register_cb
    hal_system.o(i.hal_system_reset_chip) refers to drv_crgu.o(i.drv_crgu_reset_chip) for drv_crgu_reset_chip
    hal_system.o(i.hal_system_updata_sysclk) refers to drv_crgu.o(i.drv_crgu_set_ahb_clk) for drv_crgu_set_ahb_clk
    hal_system.o(i.hal_system_updata_sysclk) refers to drv_common.o(.data) for g_system_clock
    hal_system.o(i.hal_system_updata_sysclk) refers to drv_common.o(.data) for g_system_delay_step
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_set_repeat) for drv_timer_set_repeat
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_timer.o(i.hal_timer_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_timer.o(i.hal_timer_get_status) refers to drv_timer.o(i.drv_timer_get_status) for drv_timer_get_status
    hal_timer.o(i.hal_timer_init) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_timer.o(i.hal_timer_init) refers to drv_timer.o(i.drv_timer_set_prescaler) for drv_timer_set_prescaler
    hal_timer.o(i.hal_timer_set_repeat) refers to drv_timer.o(i.drv_timer_set_repeat) for drv_timer_set_repeat
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_pwr.o(i.hal_pwr_elvcc_close) refers to drv_pwr.o(i.drv_pwr_pwmled_electric_current) for drv_pwr_pwmled_electric_current
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_pwmled_electric_current) for drv_pwr_pwmled_electric_current
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_hv_ldo_mode_sel) for drv_pwr_hv_ldo_mode_sel
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_hv_ldo_mode_clock_sel) for drv_pwr_hv_ldo_mode_clock_sel
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_pwmled_driver_current_Big_step) for drv_pwr_pwmled_driver_current_Big_step
    hal_pwr.o(i.hal_pwr_elvcc_vol_set) refers to drv_pwr.o(i.drv_pwr_hv_ldo_voltage_set) for drv_pwr_hv_ldo_voltage_set
    hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode) refers to drv_pwr.o(i.drv_pwr_set_wakeup_type) for drv_pwr_set_wakeup_type
    hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode) for drv_pwr_enter_deep_sleep_mode
    hal_pwr.o(i.hal_pwr_enter_normal_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_sleep_mode_ex) for drv_pwr_enter_sleep_mode_ex
    hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_stop_sleep_mode) for drv_pwr_enter_stop_sleep_mode
    hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) refers to hal_pwr.o(.data) for .data
    hal_pwr.o(i.hal_pwr_exit_sleep_mode) refers to drv_pwr.o(i.drv_pwr_exit_sleep_mode) for drv_pwr_exit_sleep_mode
    hal_pwr.o(i.hal_pwr_get_reset_flag) refers to drv_crgu.o(i.drv_crgu_get_all_reset_flag) for drv_crgu_get_all_reset_flag
    hal_pwr.o(i.hal_pwr_get_reset_flag) refers to drv_pwr.o(i.drv_pwr_get_wakeflag) for drv_pwr_get_wakeflag
    hal_pwr.o(i.hal_pwr_get_reset_flag) refers to drv_crgu.o(i.drv_crgu_clear_all_reset_flags) for drv_crgu_clear_all_reset_flags
    hal_pwr.o(i.hal_pwr_get_vcc_power_ready) refers to drv_pwr.o(i.drv_pwr_get_power_ready_st) for drv_pwr_get_power_ready_st
    hal_pwr.o(i.hal_pwr_ldo13s_en) refers to drv_pwr.o(i.drv_pwr_ldo13s_en) for drv_pwr_ldo13s_en
    hal_pwr.o(i.hal_pwr_ldo13s_set) refers to drv_pwr.o(i.drv_pwr_ldo13s_set) for drv_pwr_ldo13s_set
    hal_pwr.o(i.hal_pwr_ldo18s_en) refers to drv_pwr.o(i.drv_pwr_ldo18s_en) for drv_pwr_ldo18s_en
    hal_pwr.o(i.hal_pwr_ldo18s_set) refers to drv_pwr.o(i.drv_pwr_ldo18s_set) for drv_pwr_ldo18s_set
    hal_pwr.o(i.hal_pwr_set_main_power) refers to drv_pwr.o(i.drv_pwr_set_digit_power_sel) for drv_pwr_set_digit_power_sel
    hal_pwr.o(i.hal_pwr_set_pvd) refers to drv_pwr.o(i.drv_pwr_set_pvd) for drv_pwr_set_pvd
    hal_pwr.o(i.hal_pwr_set_sleep_mode_power) refers to drv_pwr.o(i.drv_pwr_set_breath_screen_power_sel) for drv_pwr_set_breath_screen_power_sel
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_ctrl_eint) for hal_gpio_ctrl_eint
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_init_eint) for hal_gpio_init_eint
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_reg_eint_cb) for hal_gpio_reg_eint_cb
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_pwr.o(.data) for .data
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_pwr.o(i.stop_sleep_cb) for stop_sleep_cb
    hal_pwr.o(i.hal_pwr_set_vcc_enable) refers to drv_pwr.o(i.drv_pwr_charge_pump_en) for drv_pwr_charge_pump_en
    hal_pwr.o(i.stop_sleep_cb) refers to hal_pwr.o(.data) for .data
    tau_delay.o(i.delayMs) refers to tau_delay.o(i.delayUs) for delayUs
    tau_delay.o(i.delayUs) refers to drv_common.o(.data) for g_system_delay_step
    tau_log.o(i.fgetc) refers to hal_uart.o(i.hal_uart_recv_blocking) for hal_uart_recv_blocking
    tau_log.o(i.fgetc) refers to hal_system.o(i.hal_system_get_debug_state) for hal_system_get_debug_state
    tau_log.o(i.fgetc) refers to hal_system.o(i.hal_system_clear_debug_state) for hal_system_clear_debug_state
    tau_log.o(i.fgetc) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.fputc) refers to tau_log.o(i.tau_log_push_log) for tau_log_push_log
    tau_log.o(i.fputc) refers to hal_uart.o(i.hal_uart_send_blocking) for hal_uart_send_blocking
    tau_log.o(i.fputc) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.tau_log_init) refers to hal_uart.o(i.hal_uart_init) for hal_uart_init
    tau_log.o(i.tau_log_init) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.tau_log_printf) refers to memseta.o(.text) for __aeabi_memclr4
    tau_log.o(i.tau_log_printf) refers to strlen.o(.text) for strlen
    tau_log.o(i.tau_log_printf) refers to printfa.o(i.__0vsprintf) for vsprintf
    tau_log.o(i.tau_log_printf) refers to tau_log.o(i.tau_log_push_log) for tau_log_push_log
    tau_log.o(i.tau_log_printf) refers to printfa.o(i.__0printf) for __2printf
    tau_log.o(i.tau_log_printf) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.tau_log_printf) refers to tau_log.o(.bss) for g_log_buf
    tau_log.o(i.tau_log_push_log) refers to memcpya.o(.text) for __aeabi_memcpy
    tau_log.o(i.tau_log_push_log) refers to tau_delay.o(i.delayUs) for delayUs
    tau_log.o(.ARM.__at_0x1101C) refers to tau_log.o(.bss) for g_log_buf
    hal_uart.o(i.hal_uart0_rx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart0_tx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart1_rx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart1_tx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_deinit) refers to drv_uart.o(i.drv_uart_deinit) for drv_uart_deinit
    hal_uart.o(i.hal_uart_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_uart.o(i.hal_uart_deinit) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_dma_path_close) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_uart.o(i.hal_uart_dma_path_close) refers to drv_dma.o(i.drv_dma_deinit) for drv_dma_deinit
    hal_uart.o(i.hal_uart_dma_path_close) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_apply_handle) for drv_dma_apply_handle
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_set_burst) for drv_dma_set_burst
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_register_callback) for drv_dma_register_callback
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_enable_int) for drv_dma_enable_int
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_set_mem_trans_info) for drv_dma_set_mem_trans_info
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_enable) for drv_dma_enable
    hal_uart.o(i.hal_uart_dma_recv) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_uart.o(i.hal_uart_dma_recv) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_dma_recv) refers to hal_uart.o(i.hal_uart0_rx_dma_cb) for hal_uart0_rx_dma_cb
    hal_uart.o(i.hal_uart_dma_recv) refers to hal_uart.o(i.hal_uart1_rx_dma_cb) for hal_uart1_rx_dma_cb
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_apply_handle) for drv_dma_apply_handle
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_set_burst) for drv_dma_set_burst
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_register_callback) for drv_dma_register_callback
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_enable_int) for drv_dma_enable_int
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_set_mem_trans_info) for drv_dma_set_mem_trans_info
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_enable) for drv_dma_enable
    hal_uart.o(i.hal_uart_dma_send) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_uart.o(i.hal_uart_dma_send) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_dma_send) refers to hal_uart.o(i.hal_uart0_tx_dma_cb) for hal_uart0_tx_dma_cb
    hal_uart.o(i.hal_uart_dma_send) refers to hal_uart.o(i.hal_uart1_tx_dma_cb) for hal_uart1_tx_dma_cb
    hal_uart.o(i.hal_uart_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_uart.o(i.hal_uart_init) refers to drv_uart.o(i.drv_uart_init) for drv_uart_init
    hal_uart.o(i.hal_uart_init) refers to drv_uart.o(i.drv_uart_trans_create_handle) for drv_uart_trans_create_handle
    hal_uart.o(i.hal_uart_init) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_init) refers to drv_common.o(.data) for g_system_clock
    hal_uart.o(i.hal_uart_init) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_recv_blocking) refers to drv_uart.o(i.drv_uart_recv_blocking) for drv_uart_recv_blocking
    hal_uart.o(i.hal_uart_recv_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_recv_none_blocking) refers to drv_uart.o(i.drv_uart_recv_none_blocking) for drv_uart_recv_none_blocking
    hal_uart.o(i.hal_uart_recv_none_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_send_blocking) refers to drv_uart.o(i.drv_uart_send_blocking) for drv_uart_send_blocking
    hal_uart.o(i.hal_uart_send_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_send_none_blocking) refers to drv_uart.o(i.drv_uart_send_none_blocking) for drv_uart_send_none_blocking
    hal_uart.o(i.hal_uart_send_none_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_internal_vsync.o(i.LCDC_IRQn_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.LCDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_internal_vsync.o(i.LCDC_IRQn_Handler) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) for hal_intl_fb_cal_fb_info
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) for hal_dsi_tx_ctrl_gen_a_tear_signal
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_delay.o(i.delayUs) for delayUs
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) for hal_vsync_reset_lcdc_scaler
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_sync_register_rx_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) for hal_intl_fb_set_fb_info_manual
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) for hal_intl_fb_cal_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_svs.o(i.hal_intl_svs_init_rx) for hal_intl_svs_init_rx
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr) for hal_intl_dcs_init_sw_fltr
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_rxbr.o(i.drv_rxbr_register_irq1_callback) for drv_rxbr_register_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_vidc.o(i.drv_vidc_register_callback) for drv_vidc_register_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_init) for dcs_packet_fifo_init
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_pro_motion_init) for soft_pro_motion_init
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_gen_te) for soft_gen_te
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.rxbr_irq1_callback) for rxbr_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.vidc_callback) for vidc_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_gen_te_double_buffer) for soft_gen_te_double_buffer
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) for hal_intl_fb_cal_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_svs.o(i.hal_intl_svs_deinit_rx) for hal_intl_svs_deinit_rx
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_svs.o(i.hal_intl_svs_set_sync_coef) for hal_intl_svs_set_sync_coef
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_memc.o(i.drv_memc_set_frame_drop_select) for drv_memc_set_frame_drop_select
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_set_tear_line) for drv_lcdc_set_tear_line
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_config_acc_command_mode) for drv_lcdc_config_acc_command_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_svs.o(i.hal_intl_svs_deinit_tx) for hal_intl_svs_deinit_tx
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.soft_pro_motion_init) for soft_pro_motion_init
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_svs.o(i.hal_intl_svs_set_input_frate) for hal_intl_svs_set_input_frate
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg) for drv_rxbr_hline_rcv0_cfg
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dadd.o(.text) for __aeabi_dadd
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_internal_vsync.o(i.soft_pro_motion_init) for soft_pro_motion_init
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_int_source) for drv_rxbr_get_int_source
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.soft_double_buffer_update) for soft_double_buffer_update
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_svs.o(i.hal_intl_svs_handle) for hal_intl_svs_handle
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.vpre_err_reset) for vpre_err_reset
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_lcdc.o(i.drv_lcdc_cmd_start) for drv_lcdc_cmd_start
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt) for hal_intl_svs_set_rx_vtt
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.soft_double_buffer_update) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(i.soft_tear_adjust_line) for soft_tear_adjust_line
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.soft_gen_te_double_buffer) refers to hal_internal_vsync.o(i.soft_tear_adjust_line) for soft_tear_adjust_line
    hal_internal_vsync.o(i.soft_gen_te_double_buffer) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_pro_motion_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.soft_pro_motion_init) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_pro_motion_init) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.soft_tear_adjust_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_get_int_source) for drv_vidc_get_int_source
    hal_internal_vsync.o(i.vidc_callback) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_clear_irq) for drv_vidc_clear_irq
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_get_irq_status) for drv_vidc_get_irq_status
    hal_internal_vsync.o(i.vidc_callback) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.vpre_err_reset) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to hal_internal_dcs.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) for hal_intl_dcs_rx_receive_packet
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_dsc_dec.o(i.drv_dsc_dec_get_nslc) for drv_dsc_dec_get_nslc
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_crgu.o(i.drv_crgu_set_dsc_clk) for drv_crgu_set_dsc_clk
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to hal_internal_dcs.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr) refers to hal_internal_dcs.o(.bss) for .bss
    hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_register_write_cmd_entry) refers to hal_internal_dcs.o(.data) for .data
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle) for hal_intl_dcs_sw_filter_handle
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) for dcs_packet_fifo_alloc
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) for hal_dsi_rx_ctrl_dcs_async_handler
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_ddi_crc_en) for drv_dsi_rx_get_ddi_crc_en
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_dcs.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_dcs.o(.data) for .data
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_dcs.o(.conststring) for .conststring
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) for hal_intl_dcs_rx_get_dcs_packet_data
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) for hal_intl_dcs_rx_receive_pps
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to hal_internal_dcs.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to memcmp.o(.text) for memcmp
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to hal_internal_dcs.o(.conststring) for .conststring
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) refers to memseta.o(.text) for __aeabi_memset
    hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) refers to drv_rxbr.o(i.drv_rxbr_set_filter_regs) for drv_rxbr_set_filter_regs
    hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) refers to hal_internal_dcs.o(.bss) for .bss
    hal_internal_dcs.o(i.hal_intl_dcs_set_dcs_direct_mode) refers to hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) for hal_intl_dcs_set_auto_hw_filter
    hal_internal_dcs.o(i.hal_intl_dcs_set_dcs_direct_mode) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle) refers to hal_internal_dcs.o(.data) for .data
    hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle) refers to hal_internal_dcs.o(.bss) for .bss
    hal_internal_dcs.o(.data) refers to hal_internal_dcs.o(.bss) for g_imm_buffer
    hal_internal_fb.o(i.ha_intl_fb_check_pu_size) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.ha_intl_fb_check_pu_size) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter) for hal_intl_fb_flow_control_adapter
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) for hal_intl_fb_check_bandwidth
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.ha_intl_fb_check_pu_size) for ha_intl_fb_check_pu_size
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.hal_intl_fb_edge_resize) for hal_intl_fb_edge_resize
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_fb.o(i.hal_intl_fb_edge_resize) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.hal_intl_fb_edge_resize) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_user_flow) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to hal_internal_fb.o(.conststring) for .conststring
    hal_internal_svs.o(i.hal_intl_svs_deinit_rx) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.hal_intl_svs_deinit_rx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_deinit_rx) refers to hal_internal_svs.o(i.svs_wait_start) for svs_wait_start
    hal_internal_svs.o(i.hal_intl_svs_deinit_tx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_handle) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) for hal_intl_svs_update_rxbr_clk
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_svs.o(i.svs_wait_start) for svs_wait_start
    hal_internal_svs.o(i.hal_intl_svs_init_tx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_svs.o(i.svs_wait_start) for svs_wait_start
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_svs.o(i.svs_wait_fr_stab) for svs_wait_fr_stab
    hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_set_sync_coef) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to dmul.o(.text) for __aeabi_dmul
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg) for drv_rxbr_hline_rcv1_cfg
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_get_rel_intv) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_svs.o(i.svs_get_rel_intv) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_sync_handle) refers to hal_internal_svs.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_svs.o(i.svs_sync_handle) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_svs.o(i.svs_sync_handle) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_svs.o(i.svs_sync_handle) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_svs.o(i.svs_sync_handle) refers to f2d.o(.text) for __aeabi_f2d
    hal_internal_svs.o(i.svs_sync_handle) refers to dadd.o(.text) for __aeabi_dadd
    hal_internal_svs.o(i.svs_sync_handle) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_svs.o(i.svs_sync_handle) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to hal_internal_svs.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to ffixui.o(.text) for __aeabi_f2uiz
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to hal_internal_svs.o(i.svs_sync_handle) for svs_sync_handle
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_svs.o(i.svs_wait_start) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_internal_svs.o(i.svs_wait_start) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_svs.o(i.svs_wait_start) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_internal_svs.o(i.svs_wait_start) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_svs.o(i.svs_wait_start) refers to f2d.o(.text) for __aeabi_f2d
    hal_internal_svs.o(i.svs_wait_start) refers to ceil.o(i.ceil) for ceil
    hal_internal_svs.o(i.svs_wait_start) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(i.svs_direct_mode_setting) for svs_direct_mode_setting
    hal_internal_svs.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_svs.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg) for drv_rxbr_hline_rcv1_cfg
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(i.svs_wait_fr_stab) for svs_wait_fr_stab
    drv_common.o(i.HardFault_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_common.o(i.SysTick_Handler) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_enable_systick) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_common.o(i.drv_common_enable_systick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_get_tick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_system_init) refers to drv_se.o(i.drv_se_init) for drv_se_init
    drv_common.o(i.drv_common_systick_register_cb) refers to drv_common.o(.data) for .data
    drv_crgu.o(i.drv_crgu_get_rxbr_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_crgu.o(i.drv_crgu_get_system_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(i.drv_dma_get_int_source) for drv_dma_get_int_source
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(i.drv_dma_clear_status) for drv_dma_clear_status
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(.data) for .data
    drv_dma.o(i.drv_dma_apply_handle) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dma.o(i.drv_dma_apply_handle) refers to drv_dma.o(.data) for .data
    drv_dma.o(i.drv_dma_apply_handle) refers to drv_dma.o(.constdata) for .constdata
    drv_dma.o(i.drv_dma_deinit) refers to drv_dma.o(i.drv_dma_disable_int) for drv_dma_disable_int
    drv_dma.o(i.drv_dma_disable_int) refers to drv_dma.o(i.drv_dma_int_list_delete) for drv_dma_int_list_delete
    drv_dma.o(i.drv_dma_disable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.drv_dma_enable_int) refers to drv_dma.o(i.drv_dma_int_list_inset) for drv_dma_int_list_inset
    drv_dma.o(i.drv_dma_enable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dma.o(i.drv_dma_init) refers to drv_per_common.o(i.drv_per_set_clock) for drv_per_set_clock
    drv_dma.o(i.drv_dma_init) refers to drv_dma.o(i.drv_dma_update_handle_setting) for drv_dma_update_handle_setting
    drv_dma.o(i.drv_dma_int_list_delete) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_int_list_inset) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_update_handle_setting) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_dma_req) for drv_sys_cfg_sel_dma_req
    drv_dma.o(i.drv_dma_update_req_by_default) refers to drv_dma.o(i.drv_dma_update_handle_setting) for drv_dma_update_handle_setting
    drv_dma.o(i.drv_dma_update_req_by_default) refers to drv_dma.o(.constdata) for .constdata
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to drv_se.o(i.drv_se_set_dsc) for drv_se_set_dsc
    drv_gpio.o(i.AP_NRESET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.AP_NRESET_IRQn_Handler) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.EXTI_INT0_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT1_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT2_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT3_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT4_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT5_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT6_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT7_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.drv_gpio_handle_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.drv_gpio_handle_int) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_register_ap_reset_callback) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.drv_gpio_register_callback) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_pwr.o(i.drv_pwr_analog_pwm_en) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_elvcc_pwm_en) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_elvcc_pwm_en) refers to tau_delay.o(i.delayMs) for delayMs
    drv_pwr.o(i.drv_pwr_enter_sleep_mode) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_enter_sleep_mode) refers to drv_pwr.o(i.drv_pwr_por_mode_flag) for drv_pwr_por_mode_flag
    drv_pwr.o(i.drv_pwr_enter_stop_sleep_mode) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_exit_sleep_mode) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_hv_ldo_mode_clock_sel) refers to drv_pwr.o(i.drv_pwr_hv_ldo_10M_clock) for drv_pwr_hv_ldo_10M_clock
    drv_pwr.o(i.drv_pwr_pwm_output_pwm_led) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_breath_screen_power_sel) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_digit_power_sel) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_system_clk) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_wakeup_type) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_spi_master.o(i.drv_spim_disable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_spi_master.o(i.drv_spim_disable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_spi_master.o(i.drv_spim_enable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_spi_master.o(i.drv_spim_enable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_spi_master.o(i.drv_spim_init) refers to drv_per_common.o(i.drv_per_get_system_clk) for drv_per_get_system_clk
    drv_spi_master.o(i.drv_spim_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_swire.o(i.SWIRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_swire.o(i.SWIRE_IRQn_Handler) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_register_callback) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_sys_cfg.o(i.drv_sys_cfg_sel_dma_req) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_timer.o(i.TIMER0_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.TIMER1_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.TIMER2_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.TIMER3_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_timer.o(i.drv_timer_enable) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_get_instance) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_get_status) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_clear_status_flags) for drv_timer_clear_status_flags
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_register_callback) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_compare_val) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_compare_val) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_timer.o(i.drv_timer_set_compare_val) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_compare_val) refers to drv_common.o(.data) for g_system_clock
    drv_timer.o(i.drv_timer_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_repeat) refers to drv_timer.o(.data) for .data
    drv_i2c.o(i.I2C0_IRQn_Handler) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.I2C1_IRQn_Handler) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.I2C2_IRQn_Handler) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_NVIC_enable) refers to drv_i2c.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_i2c.o(i.drv_i2c_NVIC_enable) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_clear_intr_status) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_i2c.o(i.drv_i2c_clear_intr_status) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_clock_enable) refers to drv_per_common.o(i.drv_per_set_clock) for drv_per_set_clock
    drv_i2c.o(i.drv_i2c_clock_enable) refers to drv_i2c.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_i2c.o(i.drv_i2c_clock_enable) refers to drv_per_common.o(i.drv_per_reset_module) for drv_per_reset_module
    drv_i2c.o(i.drv_i2c_clock_enable) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_disable_dma_req) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_disable_intr) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_enable) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_enable_dma_req) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_enable_intr) refers to drv_i2c.o(i.drv_i2c_set_sys_mask) for drv_i2c_set_sys_mask
    drv_i2c.o(i.drv_i2c_enable_intr) refers to drv_i2c.o(i.drv_i2c_clear_intr_status) for drv_i2c_clear_intr_status
    drv_i2c.o(i.drv_i2c_enable_intr) refers to drv_i2c.o(i.drv_i2c_NVIC_enable) for drv_i2c_NVIC_enable
    drv_i2c.o(i.drv_i2c_enable_intr) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_flush) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_get_fifo_status) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_get_intr_status) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_get_rx_count) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_get_tx_abrtsource) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_read_data) refers to drv_i2c.o(i.drv_i2c_get_fifo_status) for drv_i2c_get_fifo_status
    drv_i2c.o(i.drv_i2c_read_data) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_set_callback) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_set_fifo_threshold) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_set_sys_mask) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_i2c.o(i.drv_i2c_set_sys_mask) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_i2c.o(i.drv_i2c_set_sys_mask) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_write_data) refers to drv_i2c.o(i.drv_i2c_get_fifo_status) for drv_i2c_get_fifo_status
    drv_i2c.o(i.drv_i2c_write_data) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cm_cal_scl_cnt) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_i2c.o(i.drv_i2cm_cal_scl_cnt) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cm_init) refers to drv_per_common.o(i.drv_per_get_system_clk) for drv_per_get_system_clk
    drv_i2c.o(i.drv_i2cm_init) refers to drv_i2c.o(i.drv_i2cm_cal_scl_cnt) for drv_i2cm_cal_scl_cnt
    drv_i2c.o(i.drv_i2cm_init) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cm_multi_params_read_data) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cm_read_data) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cm_set_baud_rate) refers to drv_per_common.o(i.drv_per_get_system_clk) for drv_per_get_system_clk
    drv_i2c.o(i.drv_i2cm_set_baud_rate) refers to drv_i2c.o(i.drv_i2cm_cal_scl_cnt) for drv_i2cm_cal_scl_cnt
    drv_i2c.o(i.drv_i2cm_set_baud_rate) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cm_set_slave_addr) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cm_write_data) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cm_write_read_cmd) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cs_init) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cs_own_addr) refers to drv_i2c.o(.data) for .data
    drv_per_common.o(i.drv_per_get_system_clk) refers to drv_crgu.o(i.drv_crgu_get_system_clk) for drv_crgu_get_system_clk
    drv_per_common.o(i.drv_per_reset_module) refers to drv_crgu.o(i.drv_crgu_reset_modules) for drv_crgu_reset_modules
    drv_per_common.o(i.drv_per_set_clock) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_fifo_init) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_size) refers to dcs_packet_fifo.o(.bss) for .bss
    drv_se.o(i.drv_se_init) refers to drv_efuse.o(i.drv_efuse_enter_inactive) for drv_efuse_enter_inactive
    drv_se.o(i.drv_se_init) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_se.o(i.drv_se_init) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_dsc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_dsc) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_lcdc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_lcdc) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_memc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_memc) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_rxbr) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_rxbr) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_vidc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_vidc) refers to drv_se.o(.data) for .data
    drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) refers to drv_dsi_rx.o(.data) for .data
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) for drv_dsi_rx_get_color_bpp
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to ffltui.o(.text) for __aeabi_ui2f
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fdiv.o(.text) for __aeabi_fdiv
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fmul.o(.text) for __aeabi_fmul
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc) for drv_dsi_rx_get_color_pcc
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fadd.o(.text) for __aeabi_fadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to cfrcmple.o(.text) for __aeabi_cfrcmple
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to f2d.o(.text) for __aeabi_f2d
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dadd.o(.text) for __aeabi_dadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dfixui.o(.text) for __aeabi_d2uiz
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_set_drv_log_level) refers to drv_dsi_rx.o(.data) for .data
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_test_lock) for drv_phy_test_lock
    drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_enter) for drv_tx_phy_test_enter
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_code) for drv_tx_phy_test_write_code
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_exit) for drv_tx_phy_test_exit
    drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_version) for drv_dsi_tx_version
    drv_dsi_tx.o(i.drv_dsi_tx_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_tx.o(i.drv_dsi_tx_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_lcdc.o(i.drv_lcdc_clear_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_lcdc.o(i.drv_lcdc_cmd_start) refers to drv_se.o(i.drv_se_set_lcdc) for drv_se_set_lcdc
    drv_lcdc.o(i.drv_lcdc_ctrl_flow) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    drv_lcdc.o(i.drv_lcdc_part_display_config) refers to drv_lcdc.o(i.drv_lcdc_pixel_value_config) for drv_lcdc_pixel_value_config
    drv_lcdc.o(i.drv_lcdc_set_int) refers to drv_lcdc.o(i.drv_lcdc_clear_int) for drv_lcdc_clear_int
    drv_lcdc.o(i.drv_lcdc_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_lcdc.o(i.drv_lcdc_vid_hw_start) refers to drv_se.o(i.drv_se_set_lcdc) for drv_se_set_lcdc
    drv_memc.o(i.MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_get_status) for drv_memc_get_status
    drv_memc.o(i.MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_clear_status) for drv_memc_clear_status
    drv_memc.o(i.MEMC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_memc.o(i.drv_memc_rate_transfer_sel) refers to drv_se.o(i.drv_se_set_memc) for drv_se_set_memc
    drv_memc.o(i.drv_memc_set_ltpo_mode) refers to drv_se.o(i.drv_se_set_memc) for drv_se_set_memc
    drv_rxbr.o(i.VPRE1_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.VPRE1_IRQn_Handler) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_EnableIRQ) for __NVIC_EnableIRQ
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_rxbr.o(i.drv_rxbr_register_irq0_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_register_irq1_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_set_cmd_filter) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_rxbr.o(i.drv_rxbr_set_cmd_response) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_rxbr.o(i.drv_rxbr_set_color_format) refers to drv_se.o(i.drv_se_set_rxbr) for drv_se_set_rxbr
    drv_rxbr.o(i.drv_rxbr_soft_reset) refers to tau_delay.o(i.delayMs) for delayMs
    drv_rxbr.o(i.drv_rxbr_sw_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_rxbr.o(i.drv_rxbr_sw_reset) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    drv_vidc.o(i.VIDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.VIDC_IRQn_Handler) refers to drv_vidc.o(.data) for .data
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_vidc.o(i.drv_vidc_register_callback) refers to drv_vidc.o(.data) for .data
    drv_vidc.o(i.drv_vidc_set_src_parameter) refers to drv_se.o(i.drv_se_set_vidc) for drv_se_set_vidc
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_int_trans_handle) for drv_uart_int_trans_handle
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_abort_recv) for drv_uart_abort_recv
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_abort_send) for drv_uart_abort_send
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(.constdata) for .constdata
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(i.drv_uart_reset_rx_fifo) for drv_uart_reset_rx_fifo
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(i.drv_uart_reset_tx_fifo) for drv_uart_reset_tx_fifo
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_deinit) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_deinit) refers to drv_uart.o(i.drv_uart_enable_clk) for drv_uart_enable_clk
    drv_uart.o(i.drv_uart_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.drv_uart_deinit) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_enable_clk) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    drv_uart.o(i.drv_uart_enable_int) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_enable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.drv_uart_get_def_cfg) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.drv_uart_get_def_cfg) refers to drv_common.o(.data) for g_system_clock
    drv_uart.o(i.drv_uart_get_instance) refers to drv_uart.o(.constdata) for .constdata
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_enable_clk) for drv_uart_enable_clk
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_set_baud_rate) for drv_uart_set_baud_rate
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_enable_int) for drv_uart_enable_int
    drv_uart.o(i.drv_uart_int_trans_handle) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_recv_none_blocking) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_recv_none_blocking) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_recv_none_blocking) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_reset_rx_fifo) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_reset_tx_fifo) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_send_none_blocking) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_send_none_blocking) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_send_none_blocking) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_set_baud_rate) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_uart.o(i.drv_uart_trans_create_handle) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_trans_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.drv_uart_trans_create_handle) refers to drv_uart.o(.bss) for .bss
    drv_efuse.o(i.drv_efuse_enter_inactive) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    drv_efuse.o(i.drv_efuse_enter_inactive) refers to drv_efuse.o(i.drv_efuse_int_enable) for drv_efuse_int_enable
    drv_efuse.o(i.drv_efuse_read) refers to drv_pwr.o(i.drv_pwr_efuse_pd) for drv_pwr_efuse_pd
    drv_efuse.o(i.drv_efuse_read) refers to drv_efuse.o(i.drv_efuse_read_req) for drv_efuse_read_req
    drv_efuse.o(i.drv_efuse_write) refers to drv_pwr.o(i.drv_pwr_efuse_pd) for drv_pwr_efuse_pd
    drv_efuse.o(i.drv_efuse_write) refers to drv_efuse.o(i.drv_efuse_write_req) for drv_efuse_write_req
    drv_efuse.o(i.drv_efuse_write_read_req_clear) refers to drv_efuse.o(i.drv_efuse_write_req) for drv_efuse_write_req
    drv_efuse.o(i.drv_efuse_write_read_req_clear) refers to drv_efuse.o(i.drv_efuse_read_req) for drv_efuse_read_req
    ceil.o(i.__softfp_ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.__softfp_ceil) refers to ceil.o(i.ceil) for ceil
    ceil.o(i.ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.ceil) refers to dadd.o(.text) for __aeabi_dadd
    ceil.o(i.ceil) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry10a.o(.ARM.Collect$$$$0000000D) for __rt_final_cpp
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry11a.o(.ARM.Collect$$$$0000000F) for __rt_final_exit
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry7b.o(.ARM.Collect$$$$00000008) for _main_clock
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry8b.o(.ARM.Collect$$$$0000000A) for _main_cpp_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry9a.o(.ARM.Collect$$$$0000000B) for _main_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry5.o(.ARM.Collect$$$$00000004) for _main_scatterload
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry2.o(.ARM.Collect$$$$00000001) for _main_stk
    idiv.o(.text) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfb.o(i.__0fprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0fprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0printf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printfb.o(i.__0vfprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vfprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printf0.o(i.__0fprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0fprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0printf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf0.o(i.__0vfprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vfprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf1.o(i.__0fprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0fprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0printf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i.__0vfprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vfprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf2.o(i.__0fprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0fprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0printf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf2.o(i.__0vfprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vfprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf3.o(i.__0fprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0fprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0printf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i.__0vfprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vfprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf4.o(i.__0fprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0fprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0printf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i.__0vfprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vfprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf5.o(i.__0fprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0fprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0printf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i.__0vfprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vfprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf6.o(i.__0fprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0fprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0printf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i.__0vfprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vfprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i._printf_core) refers to printf6.o(i._printf_pre_padding) for _printf_pre_padding
    printf6.o(i._printf_core) refers to printf6.o(i._printf_post_padding) for _printf_post_padding
    printf6.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf7.o(i.__0fprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0fprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0printf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i.__0vfprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vfprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i._printf_core) refers to printf7.o(i._printf_pre_padding) for _printf_pre_padding
    printf7.o(i._printf_core) refers to printf7.o(i._printf_post_padding) for _printf_post_padding
    printf7.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf8.o(i.__0fprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0fprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0printf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i.__0vfprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vfprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i._printf_core) refers to printf8.o(i._printf_pre_padding) for _printf_pre_padding
    printf8.o(i._printf_core) refers to printf8.o(i._printf_post_padding) for _printf_post_padding
    printf8.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i.__0fprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0fprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0fprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0printf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0printf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0snprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0snprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0snprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0sprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0sprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0sprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i.__0vfprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vfprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vfprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0vsnprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0vsprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i._fp_digits) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._fp_digits) refers to dmul.o(.text) for __aeabi_dmul
    printfa.o(i._fp_digits) refers to ddiv.o(.text) for __aeabi_ddiv
    printfa.o(i._fp_digits) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    printfa.o(i._fp_digits) refers to dadd.o(.text) for __aeabi_dadd
    printfa.o(i._fp_digits) refers to dfixul.o(.text) for __aeabi_d2ulz
    printfa.o(i._fp_digits) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_core) refers to printfa.o(i._printf_pre_padding) for _printf_pre_padding
    printfa.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers to printfa.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i._printf_core) refers to printfa.o(i._fp_digits) for _fp_digits
    printfa.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfa.o(i._printf_post_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_pre_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._snputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._sputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    fmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers to fepilogue.o(.text) for _float_round
    fscalb.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    dadd.o(.text) refers to llsshr.o(.text) for __aeabi_lasr
    dadd.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dmul.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ddiv.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ddiv.o(.text) refers to depilogue.o(.text) for _double_round
    ffltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ffltui.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    dfltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfltui.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ffixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixui.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    f2d.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    d2f.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    d2f.o(.text) refers to fepilogue.o(.text) for _float_round
    cfcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    cfrcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    entry2.o(.ARM.Collect$$$$00000001) refers to entry2.o(.ARM.Collect$$$$00002712) for __lit__00000000
    entry2.o(.ARM.Collect$$$$00002712) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    entry5.o(.ARM.Collect$$$$00000004) refers to init.o(.text) for __scatterload
    entry9a.o(.ARM.Collect$$$$0000000B) refers to main.o(i.main) for main
    entry9b.o(.ARM.Collect$$$$0000000C) refers to main.o(i.main) for main
    uldiv.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    uldiv.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to depilogue.o(i.__ARM_clz) for __ARM_clz
    depilogue.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixul.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixul.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    init.o(.text) refers to entry5.o(.ARM.Collect$$$$00000004) for __main_after_scatterload


==============================================================================

Removing Unused input sections from the image.

    Removing main.o(.rev16_text), (4 bytes).
    Removing main.o(.revsh_text), (4 bytes).
    Removing app_tp_transfer.o(.rev16_text), (4 bytes).
    Removing app_tp_transfer.o(.revsh_text), (4 bytes).
    Removing app_tp_transfer.o(i.app_tp_i2cs_callback), (76 bytes).
    Removing app_tp_transfer.o(i.app_tp_init), (108 bytes).
    Removing app_tp_transfer.o(i.app_tp_m_read), (24 bytes).
    Removing app_tp_transfer.o(i.app_tp_m_transfer_complate), (8 bytes).
    Removing app_tp_transfer.o(i.app_tp_m_write), (28 bytes).
    Removing app_tp_transfer.o(i.app_tp_phone_clear_reset_on), (12 bytes).
    Removing app_tp_transfer.o(i.app_tp_phone_reset_init), (60 bytes).
    Removing app_tp_transfer.o(i.app_tp_phone_reset_on), (12 bytes).
    Removing app_tp_transfer.o(i.app_tp_reset_callback), (12 bytes).
    Removing app_tp_transfer.o(i.app_tp_s_read), (20 bytes).
    Removing app_tp_transfer.o(i.app_tp_s_write), (22 bytes).
    Removing app_tp_transfer.o(i.app_tp_screen_init), (60 bytes).
    Removing app_tp_transfer.o(i.app_tp_screen_int_callback), (12 bytes).
    Removing app_tp_transfer.o(i.app_tp_screen_int_init), (64 bytes).
    Removing app_tp_transfer.o(i.app_tp_screen_int_lvl_low), (28 bytes).
    Removing app_tp_transfer.o(i.app_tp_transfer_phone), (48 bytes).
    Removing app_tp_transfer.o(i.app_tp_transfer_screen_const), (256 bytes).
    Removing app_tp_transfer.o(i.app_tp_transfer_screen_int), (368 bytes).
    Removing app_tp_transfer.o(i.app_tp_transfer_screen_start), (32 bytes).
    Removing app_tp_transfer.o(i.phone_i2cs_io_init), (28 bytes).
    Removing app_tp_transfer.o(i.screen_spim_io_init), (28 bytes).
    Removing app_tp_transfer.o(.bss), (500 bytes).
    Removing app_tp_transfer.o(.constdata), (24 bytes).
    Removing app_tp_transfer.o(.data), (28 bytes).
    Removing app_tp_for_custom_s8.o(.rev16_text), (4 bytes).
    Removing app_tp_for_custom_s8.o(.revsh_text), (4 bytes).
    Removing app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data), (528 bytes).
    Removing app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const), (80 bytes).
    Removing app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int), (1152 bytes).
    Removing app_tp_for_custom_s8.o(i.app_tp_write_other_operations), (60 bytes).
    Removing app_tp_for_custom_s8.o(.bss), (142 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (1838 bytes).
    Removing app_tp_for_custom_s8.o(.data), (687 bytes).
    Removing s8_demo.o(.rev16_text), (4 bytes).
    Removing s8_demo.o(.revsh_text), (4 bytes).
    Removing s8_demo.o(i.ap_dcs_read), (232 bytes).
    Removing s8_demo.o(i.ap_dcs_set_eye_protection_mode), (100 bytes).
    Removing s8_demo.o(i.app_mipi_rx_start_cb), (80 bytes).
    Removing s8_demo.o(i.soft_swire_init), (56 bytes).
    Removing s8_demo.o(i.soft_swire_start), (46 bytes).
    Removing s8_demo.o(i.soft_swire_timer_callback), (72 bytes).
    Removing board.o(.rev16_text), (4 bytes).
    Removing board.o(.revsh_text), (4 bytes).
    Removing startup_armcm0.o(HEAP), (3072 bytes).
    Removing hal_dsi_rx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd), (220 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_short_cmd), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init), (320 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern), (260 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_force_video_crtl), (12 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en), (8 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size), (32 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback), (52 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_write_cmd_entry), (10 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle), (40 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart), (68 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd), (240 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_check_crc), (24 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk), (32 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter), (44 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_log_level), (8 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data), (240 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk), (72 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk), (56 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate), (10 bytes).
    Removing hal_dsi_tx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode), (112 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick), (244 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_frame), (12 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_get_disp_line), (12 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_overwrite_enable), (22 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_partial_disp_enable), (70 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd), (128 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle), (32 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs), (60 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm), (8 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_sync_line), (36 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect), (60 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance), (60 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness), (12 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div), (52 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc), (60 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg), (28 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera), (68 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update), (16 bytes).
    Removing hal_gpio.o(.rev16_text), (4 bytes).
    Removing hal_gpio.o(.revsh_text), (4 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_int_type), (20 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_pull_state), (40 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_driving_strength), (44 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_high_impedance), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_schmitt_trigger), (52 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_slew_rate), (52 bytes).
    Removing hal_i2c_slave.o(.rev16_text), (4 bytes).
    Removing hal_i2c_slave.o(.revsh_text), (4 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_callback), (428 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_deinit), (48 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_get_rx_cnt), (16 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_get_tx_cnt), (16 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_get_write_complete), (20 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_init), (108 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_register_callback), (16 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_rx_cnt_clear), (20 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_set_continue_transfer), (20 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_start), (96 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_stop), (84 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_tx_dma_callback), (56 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer), (88 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer), (96 bytes).
    Removing hal_i2c_slave.o(.data), (160 bytes).
    Removing hal_spi_master.o(.rev16_text), (4 bytes).
    Removing hal_spi_master.o(.revsh_text), (4 bytes).
    Removing hal_spi_master.o(i.hal_spim_deinit), (36 bytes).
    Removing hal_spi_master.o(i.hal_spim_flush), (16 bytes).
    Removing hal_spi_master.o(i.hal_spim_get_transfer_complete), (12 bytes).
    Removing hal_spi_master.o(i.hal_spim_init), (52 bytes).
    Removing hal_spi_master.o(i.hal_spim_read), (56 bytes).
    Removing hal_spi_master.o(i.hal_spim_write), (48 bytes).
    Removing hal_spi_master.o(.data), (4 bytes).
    Removing hal_spi_master.o(.data), (4 bytes).
    Removing hal_swire.o(.rev16_text), (4 bytes).
    Removing hal_swire.o(.revsh_text), (4 bytes).
    Removing hal_swire.o(i.hal_swire_register_callback), (22 bytes).
    Removing hal_swire.o(i.hal_swire_set_waveform), (92 bytes).
    Removing hal_system.o(.rev16_text), (4 bytes).
    Removing hal_system.o(.revsh_text), (4 bytes).
    Removing hal_system.o(i.hal_system_clear_debug_state), (10 bytes).
    Removing hal_system.o(i.hal_system_disable_systick), (8 bytes).
    Removing hal_system.o(i.hal_system_get_debug_state), (8 bytes).
    Removing hal_system.o(i.hal_system_idle_mode), (8 bytes).
    Removing hal_system.o(i.hal_system_register_systick_cb), (8 bytes).
    Removing hal_system.o(i.hal_system_reset_chip), (10 bytes).
    Removing hal_timer.o(.rev16_text), (4 bytes).
    Removing hal_timer.o(.revsh_text), (4 bytes).
    Removing hal_timer.o(i.hal_timer_get_status), (8 bytes).
    Removing hal_timer.o(i.hal_timer_start), (48 bytes).
    Removing hal_timer.o(i.hal_timer_start_ex), (42 bytes).
    Removing hal_timer.o(i.hal_timer_stop), (40 bytes).
    Removing hal_pwr.o(.rev16_text), (4 bytes).
    Removing hal_pwr.o(.revsh_text), (4 bytes).
    Removing hal_pwr.o(i.hal_pwr_elvcc_close), (10 bytes).
    Removing hal_pwr.o(i.hal_pwr_elvcc_ldo_en), (46 bytes).
    Removing hal_pwr.o(i.hal_pwr_elvcc_vol_set), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_get_reset_flag), (66 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo13s_en), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo13s_set), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo18s_en), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo18s_set), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_set_vcc_enable), (8 bytes).
    Removing tau_delay.o(.rev16_text), (4 bytes).
    Removing tau_delay.o(.revsh_text), (4 bytes).
    Removing tau_log.o(.rev16_text), (4 bytes).
    Removing tau_log.o(.revsh_text), (4 bytes).
    Removing tau_log.o(i.fgetc), (72 bytes).
    Removing hal_uart.o(.rev16_text), (4 bytes).
    Removing hal_uart.o(.revsh_text), (4 bytes).
    Removing hal_uart.o(i.hal_uart0_rx_dma_cb), (20 bytes).
    Removing hal_uart.o(i.hal_uart0_tx_dma_cb), (36 bytes).
    Removing hal_uart.o(i.hal_uart1_rx_dma_cb), (20 bytes).
    Removing hal_uart.o(i.hal_uart1_tx_dma_cb), (36 bytes).
    Removing hal_uart.o(i.hal_uart_deinit), (48 bytes).
    Removing hal_uart.o(i.hal_uart_dma_path_close), (92 bytes).
    Removing hal_uart.o(i.hal_uart_dma_recv), (276 bytes).
    Removing hal_uart.o(i.hal_uart_dma_send), (280 bytes).
    Removing hal_uart.o(i.hal_uart_recv_blocking), (28 bytes).
    Removing hal_uart.o(i.hal_uart_recv_none_blocking), (28 bytes).
    Removing hal_uart.o(i.hal_uart_send_none_blocking), (28 bytes).
    Removing hal_internal_vsync.o(.rev16_text), (4 bytes).
    Removing hal_internal_vsync.o(.revsh_text), (4 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te), (2 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_register_rx_callback), (28 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual), (28 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line), (60 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate), (134 bytes).
    Removing hal_internal_vsync.o(.data), (4 bytes).
    Removing hal_internal_dcs.o(.rev16_text), (4 bytes).
    Removing hal_internal_dcs.o(.revsh_text), (4 bytes).
    Removing hal_internal_dcs.o(i.hal_intl_dcs_register_write_cmd_entry), (12 bytes).
    Removing hal_internal_dcs.o(i.hal_intl_dcs_set_dcs_direct_mode), (44 bytes).
    Removing hal_internal_fb.o(.rev16_text), (4 bytes).
    Removing hal_internal_fb.o(.revsh_text), (4 bytes).
    Removing hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual), (480 bytes).
    Removing hal_internal_fb.o(.conststring), (152 bytes).
    Removing hal_internal_svs.o(.rev16_text), (4 bytes).
    Removing hal_internal_svs.o(.revsh_text), (4 bytes).
    Removing hal_internal_svs.o(i.hal_intl_svs_set_input_frate), (112 bytes).
    Removing hal_internal_svs.o(i.hal_intl_svs_set_sync_coef), (12 bytes).
    Removing drv_common.o(.rev16_text), (4 bytes).
    Removing drv_common.o(.revsh_text), (4 bytes).
    Removing drv_common.o(i.drv_common_disable_systick), (20 bytes).
    Removing drv_common.o(i.drv_common_idle_mode), (40 bytes).
    Removing drv_common.o(i.drv_common_systick_register_cb), (12 bytes).
    Removing drv_crgu.o(.rev16_text), (4 bytes).
    Removing drv_crgu.o(.revsh_text), (4 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_all_reset_flags), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_reset_flag), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_all_reset_flag), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_reset_flag), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_system_clk), (104 bytes).
    Removing drv_crgu.o(i.drv_crgu_reset_chip), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_clock_src), (16 bytes).
    Removing drv_dma.o(.rev16_text), (4 bytes).
    Removing drv_dma.o(.revsh_text), (4 bytes).
    Removing drv_dma.o(i.drv_dma_apply_handle), (304 bytes).
    Removing drv_dma.o(i.drv_dma_deinit), (52 bytes).
    Removing drv_dma.o(i.drv_dma_disable), (20 bytes).
    Removing drv_dma.o(i.drv_dma_disable_int), (40 bytes).
    Removing drv_dma.o(i.drv_dma_enable), (36 bytes).
    Removing drv_dma.o(i.drv_dma_enable_int), (68 bytes).
    Removing drv_dma.o(i.drv_dma_get_remaining_trans_num), (20 bytes).
    Removing drv_dma.o(i.drv_dma_get_status), (20 bytes).
    Removing drv_dma.o(i.drv_dma_init), (22 bytes).
    Removing drv_dma.o(i.drv_dma_int_list_delete), (88 bytes).
    Removing drv_dma.o(i.drv_dma_int_list_inset), (48 bytes).
    Removing drv_dma.o(i.drv_dma_register_callback), (4 bytes).
    Removing drv_dma.o(i.drv_dma_reset), (36 bytes).
    Removing drv_dma.o(i.drv_dma_set_bitwide), (56 bytes).
    Removing drv_dma.o(i.drv_dma_set_burst), (20 bytes).
    Removing drv_dma.o(i.drv_dma_set_circle_mode), (40 bytes).
    Removing drv_dma.o(i.drv_dma_set_dir), (40 bytes).
    Removing drv_dma.o(i.drv_dma_set_increment), (72 bytes).
    Removing drv_dma.o(i.drv_dma_set_mem_trans_info), (40 bytes).
    Removing drv_dma.o(i.drv_dma_set_mem_trans_offset), (24 bytes).
    Removing drv_dma.o(i.drv_dma_set_per_address), (20 bytes).
    Removing drv_dma.o(i.drv_dma_set_priority), (32 bytes).
    Removing drv_dma.o(i.drv_dma_set_tran_int_cnt), (28 bytes).
    Removing drv_dma.o(i.drv_dma_update_handle_setting), (148 bytes).
    Removing drv_dma.o(i.drv_dma_update_req_by_default), (40 bytes).
    Removing drv_dma.o(.constdata), (136 bytes).
    Removing drv_dsc_dec.o(.rev16_text), (4 bytes).
    Removing drv_dsc_dec.o(.revsh_text), (4 bytes).
    Removing drv_gpio.o(.rev16_text), (4 bytes).
    Removing drv_gpio.o(.revsh_text), (4 bytes).
    Removing drv_pwr.o(.rev16_text), (4 bytes).
    Removing drv_pwr.o(.revsh_text), (4 bytes).
    Removing drv_pwr.o(i.drv_pwr_10bit_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_analog_pwm_en), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_charge_pump_en), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_close_iov18_tp18), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_dsc_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_elvcc_pwm_en), (124 bytes).
    Removing drv_pwr.o(i.drv_pwr_enter_sleep_mode), (152 bytes).
    Removing drv_pwr.o(i.drv_pwr_exit_sleep_mode_ex), (40 bytes).
    Removing drv_pwr.o(i.drv_pwr_fb_pd), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_get_wakeflag), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_get_write_lock_st), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_hf_frm_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_10M_clock), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_mode_clock_sel), (60 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_mode_sel), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_voltage_set), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo11d_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo13s_en), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo13s_set), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo15_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo18s_en), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo18s_set), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_ltpo_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_osc32k_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_osc80m_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_p3k_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_por_mode_flag), (32 bytes).
    Removing drv_pwr.o(i.drv_pwr_power_in), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_power_ready_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_power_sel), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwm_output_pwm_led), (56 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_driver_current_Big_step), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_driver_current_small_step), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_electric_current), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_open_drain), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_ram_pd_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_read_boot_chipst), (12 bytes).
    Removing drv_pwr.o(i.drv_pwr_read_chipcfg), (12 bytes).
    Removing drv_pwr.o(i.drv_pwr_rgbr_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_ap_rst_mode), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_ldo11_mode), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_ldo15_mode), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_pvd_mode), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_system_clk), (32 bytes).
    Removing drv_pwr.o(i.drv_pwr_sw_tp18_en), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_wakeflag_get), (16 bytes).
    Removing drv_spi_master.o(.rev16_text), (4 bytes).
    Removing drv_spi_master.o(.revsh_text), (4 bytes).
    Removing drv_spi_master.o(i.drv_spim_enable_int), (40 bytes).
    Removing drv_spi_master.o(i.drv_spim_init), (100 bytes).
    Removing drv_spi_master.o(i.drv_spim_read), (104 bytes).
    Removing drv_spi_master.o(i.drv_spim_write), (64 bytes).
    Removing drv_swire.o(.rev16_text), (4 bytes).
    Removing drv_swire.o(.revsh_text), (4 bytes).
    Removing drv_sys_cfg.o(.rev16_text), (4 bytes).
    Removing drv_sys_cfg.o(.revsh_text), (4 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_sel_dma_req), (128 bytes).
    Removing drv_timer.o(.rev16_text), (4 bytes).
    Removing drv_timer.o(.revsh_text), (4 bytes).
    Removing drv_timer.o(i.drv_timer_get_status), (38 bytes).
    Removing drv_timer.o(i.drv_timer_register_callback), (20 bytes).
    Removing drv_i2c.o(.rev16_text), (4 bytes).
    Removing drv_i2c.o(.revsh_text), (4 bytes).
    Removing drv_i2c.o(i.__NVIC_DisableIRQ), (32 bytes).
    Removing drv_i2c.o(i.drv_i2c_NVIC_enable), (52 bytes).
    Removing drv_i2c.o(i.drv_i2c_clear_intr_status), (72 bytes).
    Removing drv_i2c.o(i.drv_i2c_clock_enable), (52 bytes).
    Removing drv_i2c.o(i.drv_i2c_disable_dma_req), (24 bytes).
    Removing drv_i2c.o(i.drv_i2c_disable_intr), (20 bytes).
    Removing drv_i2c.o(i.drv_i2c_enable), (36 bytes).
    Removing drv_i2c.o(i.drv_i2c_enable_dma_req), (24 bytes).
    Removing drv_i2c.o(i.drv_i2c_enable_intr), (56 bytes).
    Removing drv_i2c.o(i.drv_i2c_flush), (24 bytes).
    Removing drv_i2c.o(i.drv_i2c_get_fifo_status), (36 bytes).
    Removing drv_i2c.o(i.drv_i2c_get_intr_status), (16 bytes).
    Removing drv_i2c.o(i.drv_i2c_get_rx_count), (20 bytes).
    Removing drv_i2c.o(i.drv_i2c_get_tx_abrtsource), (20 bytes).
    Removing drv_i2c.o(i.drv_i2c_read_data), (44 bytes).
    Removing drv_i2c.o(i.drv_i2c_set_callback), (16 bytes).
    Removing drv_i2c.o(i.drv_i2c_set_fifo_threshold), (32 bytes).
    Removing drv_i2c.o(i.drv_i2c_set_sys_mask), (48 bytes).
    Removing drv_i2c.o(i.drv_i2c_write_data), (40 bytes).
    Removing drv_i2c.o(i.drv_i2cm_cal_scl_cnt), (40 bytes).
    Removing drv_i2c.o(i.drv_i2cm_init), (156 bytes).
    Removing drv_i2c.o(i.drv_i2cm_multi_params_read_data), (132 bytes).
    Removing drv_i2c.o(i.drv_i2cm_read_data), (140 bytes).
    Removing drv_i2c.o(i.drv_i2cm_set_baud_rate), (76 bytes).
    Removing drv_i2c.o(i.drv_i2cm_set_slave_addr), (52 bytes).
    Removing drv_i2c.o(i.drv_i2cm_write_data), (76 bytes).
    Removing drv_i2c.o(i.drv_i2cm_write_read_cmd), (60 bytes).
    Removing drv_i2c.o(i.drv_i2cs_init), (72 bytes).
    Removing drv_i2c.o(i.drv_i2cs_own_addr), (16 bytes).
    Removing drv_per_common.o(.rev16_text), (4 bytes).
    Removing drv_per_common.o(.revsh_text), (4 bytes).
    Removing drv_per_common.o(i.drv_per_get_system_clk), (8 bytes).
    Removing drv_per_common.o(i.drv_per_reset_module), (14 bytes).
    Removing drv_per_common.o(i.drv_per_set_clock), (14 bytes).
    Removing dcs_packet_fifo.o(.rev16_text), (4 bytes).
    Removing dcs_packet_fifo.o(.revsh_text), (4 bytes).
    Removing dcs_packet_fifo.o(i.dcs_packet_get_fifo_size), (16 bytes).
    Removing drv_se.o(.rev16_text), (4 bytes).
    Removing drv_se.o(.revsh_text), (4 bytes).
    Removing drv_dsi_rx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_rx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_force_video_crtl), (28 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_lpdt_fifo_status), (16 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size), (12 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate), (68 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_version), (12 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg), (24 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_drv_log_level), (12 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg), (48 bytes).
    Removing drv_dsi_tx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_tx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_force_interrupt), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_get_phy_status), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_forcepll), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_start), (24 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot), (68 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger), (92 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter), (296 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit), (228 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_sdf_3d), (32 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_bta), (28 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_vpg), (100 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_version), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_vid_shadow), (20 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_clear), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_lock), (32 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_read), (16 bytes).
    Removing drv_lcdc.o(.rev16_text), (4 bytes).
    Removing drv_lcdc.o(.revsh_text), (4 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_clear_irq), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_dpisignal_output_ctrl), (44 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_fixed_frame_output), (56 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_dpbuf_num), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_dpi_status), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_frame_clk_count), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_int_en_status), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_int_status), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_line_status), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_rgb2pen_subpixel), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_part_display_config), (52 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_pixel_value_config), (32 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_rd_st_line_config), (28 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_software_reset), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_update_shadow_reg), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_vid_sw_start), (56 bytes).
    Removing drv_memc.o(.rev16_text), (4 bytes).
    Removing drv_memc.o(.revsh_text), (4 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_frm_time), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_int_frame), (36 bytes).
    Removing drv_memc.o(i.drv_memc_set_double_buffer_reverse), (24 bytes).
    Removing drv_memc.o(i.drv_memc_set_fb_pri), (44 bytes).
    Removing drv_memc.o(i.drv_memc_set_fb_remaining_line_trigger), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_inten), (28 bytes).
    Removing drv_memc.o(i.drv_memc_set_read_trigger_line), (24 bytes).
    Removing drv_memc.o(i.drv_memc_set_te_ind), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_tear_hwclr), (24 bytes).
    Removing drv_memc.o(i.drv_memc_set_vidc_fb_arb), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_write_trigger_line), (24 bytes).
    Removing drv_rxbr.o(.rev16_text), (4 bytes).
    Removing drv_rxbr.o(.revsh_text), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_clr_swp_cnt), (16 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_dsc_flush), (24 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_col_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_cur_hline_rcv_cnt), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_frame_data_interval), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_hline_dcat), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_ipi_vsync_interval), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_page_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_pix_fmt), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_swpxl_cnt), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg), (20 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_register_irq0_callback), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header), (24 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_ack_pkt_md), (28 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_cmd_filter), (320 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_col_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_compress), (32 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_data_catch_hline), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_page_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_swpxl_data), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_tmpdith_bp), (28 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_soft_reset), (32 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_sw_reset), (164 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_swpxl_clr), (32 bytes).
    Removing drv_vidc.o(.rev16_text), (4 bytes).
    Removing drv_vidc.o(.revsh_text), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_clear_status0), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_cap_pixel), (28 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_signal_frame), (36 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status0), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status1), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status2), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_dsc_thresh), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_frmst_latency), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_inff_thresh), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_irq_line), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_module_enable), (28 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_outff_thresh), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_update_src_format), (20 bytes).
    Removing drv_uart.o(.rev16_text), (4 bytes).
    Removing drv_uart.o(.revsh_text), (4 bytes).
    Removing drv_uart.o(i.drv_uart_deinit), (60 bytes).
    Removing drv_uart.o(i.drv_uart_get_def_cfg), (72 bytes).
    Removing drv_uart.o(i.drv_uart_recv_blocking), (48 bytes).
    Removing drv_uart.o(i.drv_uart_recv_none_blocking), (60 bytes).
    Removing drv_uart.o(i.drv_uart_send_none_blocking), (60 bytes).
    Removing drv_efuse.o(.rev16_text), (4 bytes).
    Removing drv_efuse.o(.revsh_text), (4 bytes).
    Removing drv_efuse.o(i.drv_efuse_crc_cal), (128 bytes).
    Removing drv_efuse.o(i.drv_efuse_get_default_config), (26 bytes).
    Removing drv_efuse.o(i.drv_efuse_int_disable), (12 bytes).
    Removing drv_efuse.o(i.drv_efuse_write), (56 bytes).
    Removing drv_efuse.o(i.drv_efuse_write_read_req_clear), (22 bytes).
    Removing drv_efuse.o(i.drv_efuse_write_req), (22 bytes).
    Removing drv_phy_common.o(.rev16_text), (4 bytes).
    Removing drv_phy_common.o(.revsh_text), (4 bytes).

463 unused section(s) (total 26835 bytes) removed from the image.

==============================================================================

Image Symbol Table

    Local Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    ../clib/../cmprslib/zerorunl2.c          0x00000000   Number         0  __dczerorl2.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uidiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  idiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uldiv.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry5.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry2.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7b.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llushr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llsshr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llshl.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf6.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf7.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfa.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfb.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf0.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf1.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf2.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf3.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf8.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf4.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf5.o ABSOLUTE
    ../clib/microlib/printf/stubs.s          0x00000000   Number         0  stubs.o ABSOLUTE
    ../clib/microlib/stdio/streams.c         0x00000000   Number         0  stdout.o ABSOLUTE
    ../clib/microlib/string/memcmp.c         0x00000000   Number         0  memcmp.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpyb.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpya.o ABSOLUTE
    ../clib/microlib/string/memset.c         0x00000000   Number         0  memseta.o ABSOLUTE
    ../clib/microlib/string/strlen.c         0x00000000   Number         0  strlen.o ABSOLUTE
    ../clib/microlib/stubs.s                 0x00000000   Number         0  iusefp.o ABSOLUTE
    ../fplib/microlib/d2f.c                  0x00000000   Number         0  d2f.o ABSOLUTE
    ../fplib/microlib/f2d.c                  0x00000000   Number         0  f2d.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  fadd.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  dadd.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  ddiv.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  fdiv.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  fepilogue.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  depilogue.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  ffixui.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixui.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixul.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  ffltui.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  dfltui.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  fmul.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  dmul.o ABSOLUTE
    ../fplib/microlib/fpscalb.c              0x00000000   Number         0  fscalb.o ABSOLUTE
    ../mathlib/ceil.c                        0x00000000   Number         0  ceil.o ABSOLUTE
    ..\..\..\src\common\tau_delay.c          0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\..\..\src\common\tau_log.c            0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_i2c.c 0x00000000   Number         0  drv_i2c.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_per_common.c 0x00000000   Number         0  drv_per_common.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_spi_master.c 0x00000000   Number         0  drv_spi_master.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_i2c_slave.c 0x00000000   Number         0  hal_i2c_slave.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_pwr.c 0x00000000   Number         0  hal_pwr.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_spi_master.c 0x00000000   Number         0  hal_spi_master.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_swire.c 0x00000000   Number         0  hal_swire.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_timer.c 0x00000000   Number         0  hal_timer.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\dcs_packet_fifo.c 0x00000000   Number         0  dcs_packet_fifo.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_dcs.c 0x00000000   Number         0  hal_internal_dcs.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_fb.c 0x00000000   Number         0  hal_internal_fb.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_svs.c 0x00000000   Number         0  hal_internal_svs.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\src\drv_se.c  0x00000000   Number         0  drv_se.o ABSOLUTE
    ..\..\src\app\S8\app_tp_for_custom_s8.c  0x00000000   Number         0  app_tp_for_custom_s8.o ABSOLUTE
    ..\..\src\app\S8\s8_demo.c               0x00000000   Number         0  s8_demo.o ABSOLUTE
    ..\..\src\app\main.c                     0x00000000   Number         0  main.o ABSOLUTE
    ..\..\src\app\touch\app_tp_transfer.c    0x00000000   Number         0  app_tp_transfer.o ABSOLUTE
    ..\..\src\board\board.c                  0x00000000   Number         0  board.o ABSOLUTE
    ..\..\src\board\startup\startup_ARMCM0.s 0x00000000   Number         0  startup_armcm0.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_delay.c     0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_log.c       0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_i2c.c 0x00000000   Number         0  drv_i2c.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_per_common.c 0x00000000   Number         0  drv_per_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_spi_master.c 0x00000000   Number         0  drv_spi_master.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_i2c_slave.c 0x00000000   Number         0  hal_i2c_slave.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_pwr.c 0x00000000   Number         0  hal_pwr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_spi_master.c 0x00000000   Number         0  hal_spi_master.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_swire.c 0x00000000   Number         0  hal_swire.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_timer.c 0x00000000   Number         0  hal_timer.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\dcs_packet_fifo.c 0x00000000   Number         0  dcs_packet_fifo.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_dcs.c 0x00000000   Number         0  hal_internal_dcs.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_fb.c 0x00000000   Number         0  hal_internal_fb.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_svs.c 0x00000000   Number         0  hal_internal_svs.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\src\\drv_se.c 0x00000000   Number         0  drv_se.o ABSOLUTE
    ..\\..\\src\\app\\S8\\app_tp_for_custom_s8.c 0x00000000   Number         0  app_tp_for_custom_s8.o ABSOLUTE
    ..\\..\\src\\app\\S8\\s8_demo.c          0x00000000   Number         0  s8_demo.o ABSOLUTE
    ..\\..\\src\\app\\main.c                 0x00000000   Number         0  main.o ABSOLUTE
    ..\\..\\src\\app\\touch\\app_tp_transfer.c 0x00000000   Number         0  app_tp_transfer.o ABSOLUTE
    ..\\..\\src\\board\\board.c              0x00000000   Number         0  board.o ABSOLUTE
    cdrcmple.s                               0x00000000   Number         0  cdrcmple.o ABSOLUTE
    cfcmple.s                                0x00000000   Number         0  cfcmple.o ABSOLUTE
    cfrcmple.s                               0x00000000   Number         0  cfrcmple.o ABSOLUTE
    dc.s                                     0x00000000   Number         0  dc.o ABSOLUTE
    handlers.s                               0x00000000   Number         0  handlers.o ABSOLUTE
    init.s                                   0x00000000   Number         0  init.o ABSOLUTE
    RESET                                    0x00010000   Section      192  startup_armcm0.o(RESET)
    .ARM.Collect$$$$00000000                 0x000100c0   Section        0  entry.o(.ARM.Collect$$$$00000000)
    .ARM.Collect$$$$00000001                 0x000100c0   Section        4  entry2.o(.ARM.Collect$$$$00000001)
    .ARM.Collect$$$$00000004                 0x000100c4   Section        4  entry5.o(.ARM.Collect$$$$00000004)
    .ARM.Collect$$$$00000008                 0x000100c8   Section        0  entry7b.o(.ARM.Collect$$$$00000008)
    .ARM.Collect$$$$0000000A                 0x000100c8   Section        0  entry8b.o(.ARM.Collect$$$$0000000A)
    .ARM.Collect$$$$0000000B                 0x000100c8   Section        8  entry9a.o(.ARM.Collect$$$$0000000B)
    .ARM.Collect$$$$0000000D                 0x000100d0   Section        0  entry10a.o(.ARM.Collect$$$$0000000D)
    .ARM.Collect$$$$0000000F                 0x000100d0   Section        0  entry11a.o(.ARM.Collect$$$$0000000F)
    .ARM.Collect$$$$00002712                 0x000100d0   Section        4  entry2.o(.ARM.Collect$$$$00002712)
    __lit__00000000                          0x000100d0   Data           4  entry2.o(.ARM.Collect$$$$00002712)
    .text                                    0x000100d4   Section      120  startup_armcm0.o(.text)
    .text                                    0x0001014c   Section        0  uidiv.o(.text)
    .text                                    0x00010178   Section        0  idiv.o(.text)
    .text                                    0x000101a0   Section        0  memcpya.o(.text)
    .text                                    0x000101c4   Section        0  memseta.o(.text)
    .text                                    0x000101e8   Section        0  strlen.o(.text)
    .text                                    0x000101f6   Section        0  memcmp.o(.text)
    .text                                    0x00010210   Section        0  fadd.o(.text)
    .text                                    0x000102c2   Section        0  fmul.o(.text)
    .text                                    0x0001033c   Section        0  fdiv.o(.text)
    .text                                    0x000103b8   Section        0  fscalb.o(.text)
    .text                                    0x000103d0   Section        0  dadd.o(.text)
    .text                                    0x00010534   Section        0  dmul.o(.text)
    .text                                    0x00010604   Section        0  ddiv.o(.text)
    .text                                    0x000106f4   Section        0  ffltui.o(.text)
    .text                                    0x00010704   Section        0  dfltui.o(.text)
    .text                                    0x00010720   Section        0  ffixui.o(.text)
    .text                                    0x00010748   Section        0  dfixui.o(.text)
    .text                                    0x00010784   Section        0  f2d.o(.text)
    .text                                    0x000107ac   Section        0  d2f.o(.text)
    .text                                    0x000107e4   Section       20  cfcmple.o(.text)
    .text                                    0x000107f8   Section       20  cfrcmple.o(.text)
    .text                                    0x0001080c   Section        0  uldiv.o(.text)
    .text                                    0x0001086c   Section        0  llshl.o(.text)
    .text                                    0x0001088c   Section        0  llushr.o(.text)
    .text                                    0x000108ae   Section        0  llsshr.o(.text)
    .text                                    0x000108d4   Section        0  fepilogue.o(.text)
    .text                                    0x000108d4   Section        0  iusefp.o(.text)
    .text                                    0x00010956   Section        0  depilogue.o(.text)
    .text                                    0x00010a14   Section        0  dfixul.o(.text)
    .text                                    0x00010a54   Section       40  cdrcmple.o(.text)
    .text                                    0x00010a7c   Section       36  init.o(.text)
    .text                                    0x00010aa0   Section        0  __dczerorl2.o(.text)
    i.AP_NRESET_IRQn_Handler                 0x00010af8   Section        0  drv_gpio.o(i.AP_NRESET_IRQn_Handler)
    i.DMA_IRQn_Handler                       0x00010b14   Section        0  drv_dma.o(i.DMA_IRQn_Handler)
    i.EXTI_INT0_IRQn_Handler                 0x00010b70   Section        0  drv_gpio.o(i.EXTI_INT0_IRQn_Handler)
    i.EXTI_INT1_IRQn_Handler                 0x00010b7a   Section        0  drv_gpio.o(i.EXTI_INT1_IRQn_Handler)
    i.EXTI_INT2_IRQn_Handler                 0x00010b84   Section        0  drv_gpio.o(i.EXTI_INT2_IRQn_Handler)
    i.EXTI_INT3_IRQn_Handler                 0x00010b8e   Section        0  drv_gpio.o(i.EXTI_INT3_IRQn_Handler)
    i.EXTI_INT4_IRQn_Handler                 0x00010b98   Section        0  drv_gpio.o(i.EXTI_INT4_IRQn_Handler)
    i.EXTI_INT5_IRQn_Handler                 0x00010ba2   Section        0  drv_gpio.o(i.EXTI_INT5_IRQn_Handler)
    i.EXTI_INT6_IRQn_Handler                 0x00010bac   Section        0  drv_gpio.o(i.EXTI_INT6_IRQn_Handler)
    i.EXTI_INT7_IRQn_Handler                 0x00010bb6   Section        0  drv_gpio.o(i.EXTI_INT7_IRQn_Handler)
    i.HardFault_Handler                      0x00010bc0   Section        0  drv_common.o(i.HardFault_Handler)
    i.I2C0_IRQn_Handler                      0x00010c08   Section        0  drv_i2c.o(i.I2C0_IRQn_Handler)
    i.I2C1_IRQn_Handler                      0x00010c14   Section        0  drv_i2c.o(i.I2C1_IRQn_Handler)
    i.I2C2_IRQn_Handler                      0x00010c20   Section        0  drv_i2c.o(i.I2C2_IRQn_Handler)
    i.LCDC_IRQn_Handler                      0x00010c2c   Section        0  hal_internal_vsync.o(i.LCDC_IRQn_Handler)
    i.MEMC_IRQn_Handler                      0x00010d2c   Section        0  drv_memc.o(i.MEMC_IRQn_Handler)
    i.MIPI_TX_IRQn_Handler                   0x00010dc8   Section        0  drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler)
    i.PhoneDisOffDeal                        0x00010e80   Section        0  s8_demo.o(i.PhoneDisOffDeal)
    PhoneDisOffDeal                          0x00010e81   Thumb Code   172  s8_demo.o(i.PhoneDisOffDeal)
    i.SPIM_IRQn_Handler                      0x00010f34   Section        0  hal_spi_master.o(i.SPIM_IRQn_Handler)
    i.SWIRE_IRQn_Handler                     0x00010f7c   Section        0  drv_swire.o(i.SWIRE_IRQn_Handler)
    i.SysTick_Handler                        0x00010fac   Section        0  drv_common.o(i.SysTick_Handler)
    i.TIMER0_IRQn_Handler                    0x00010fc4   Section        0  drv_timer.o(i.TIMER0_IRQn_Handler)
    i.TIMER1_IRQn_Handler                    0x00010fce   Section        0  drv_timer.o(i.TIMER1_IRQn_Handler)
    i.TIMER2_IRQn_Handler                    0x00010fd8   Section        0  drv_timer.o(i.TIMER2_IRQn_Handler)
    i.TIMER3_IRQn_Handler                    0x00010fe2   Section        0  drv_timer.o(i.TIMER3_IRQn_Handler)
    i.__scatterload_copy                     0x00010fec   Section       14  handlers.o(i.__scatterload_copy)
    i.__scatterload_null                     0x00010ffa   Section        2  handlers.o(i.__scatterload_null)
    .ARM.__at_0x11000                        0x00011000   Section       28  drv_common.o(.ARM.__at_0x11000)
    .ARM.__at_0x1101C                        0x0001101c   Section       16  tau_log.o(.ARM.__at_0x1101C)
    .ARM.__at_0x1102C                        0x0001102c   Section       22  hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C)
    i.MIPI_RX_IRQn_Handler                   0x00011044   Section        0  drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler)
    i.UART_IRQn_Handler                      0x000113a8   Section        0  drv_uart.o(i.UART_IRQn_Handler)
    i.VIDC_IRQn_Handler                      0x00011528   Section        0  drv_vidc.o(i.VIDC_IRQn_Handler)
    i.VPRE1_IRQn_Handler                     0x00011544   Section        0  drv_rxbr.o(i.VPRE1_IRQn_Handler)
    i.VPRE_IRQn_Handler                      0x00011560   Section        0  hal_internal_dcs.o(i.VPRE_IRQn_Handler)
    i.__0printf                              0x000115cc   Section        0  printfa.o(i.__0printf)
    i.__0vsprintf                            0x000115ec   Section        0  printfa.o(i.__0vsprintf)
    i.__ARM_clz                              0x00011610   Section        0  depilogue.o(i.__ARM_clz)
    i.__ARM_common_switch8                   0x0001163e   Section        0  hal_dsi_rx_ctrl.o(i.__ARM_common_switch8)
    i.__NVIC_DisableIRQ                      0x00011658   Section        0  drv_rxbr.o(i.__NVIC_DisableIRQ)
    __NVIC_DisableIRQ                        0x00011659   Thumb Code    26  drv_rxbr.o(i.__NVIC_DisableIRQ)
    i.__NVIC_EnableIRQ                       0x00011678   Section        0  drv_rxbr.o(i.__NVIC_EnableIRQ)
    __NVIC_EnableIRQ                         0x00011679   Thumb Code    18  drv_rxbr.o(i.__NVIC_EnableIRQ)
    i.__scatterload_zeroinit                 0x00011690   Section       14  handlers.o(i.__scatterload_zeroinit)
    i._fp_digits                             0x000116a0   Section        0  printfa.o(i._fp_digits)
    _fp_digits                               0x000116a1   Thumb Code   344  printfa.o(i._fp_digits)
    i._printf_core                           0x00011814   Section        0  printfa.o(i._printf_core)
    _printf_core                             0x00011815   Thumb Code  1754  printfa.o(i._printf_core)
    i._printf_post_padding                   0x00011f00   Section        0  printfa.o(i._printf_post_padding)
    _printf_post_padding                     0x00011f01   Thumb Code    32  printfa.o(i._printf_post_padding)
    i._printf_pre_padding                    0x00011f20   Section        0  printfa.o(i._printf_pre_padding)
    _printf_pre_padding                      0x00011f21   Thumb Code    44  printfa.o(i._printf_pre_padding)
    i._sputc                                 0x00011f4c   Section        0  printfa.o(i._sputc)
    _sputc                                   0x00011f4d   Thumb Code    10  printfa.o(i._sputc)
    i.ap_dcs_set_AOD_53                      0x00011f58   Section        0  s8_demo.o(i.ap_dcs_set_AOD_53)
    ap_dcs_set_AOD_53                        0x00011f59   Thumb Code    28  s8_demo.o(i.ap_dcs_set_AOD_53)
    i.ap_dcs_set_backlight                   0x00011f78   Section        0  s8_demo.o(i.ap_dcs_set_backlight)
    ap_dcs_set_backlight                     0x00011f79   Thumb Code   170  s8_demo.o(i.ap_dcs_set_backlight)
    i.ap_dcs_set_display_off                 0x00012038   Section        0  s8_demo.o(i.ap_dcs_set_display_off)
    ap_dcs_set_display_off                   0x00012039   Thumb Code     6  s8_demo.o(i.ap_dcs_set_display_off)
    i.ap_dcs_set_display_on                  0x00012040   Section        0  s8_demo.o(i.ap_dcs_set_display_on)
    ap_dcs_set_display_on                    0x00012041   Thumb Code    28  s8_demo.o(i.ap_dcs_set_display_on)
    i.ap_dcs_set_enter_sleep_mode            0x0001207c   Section        0  s8_demo.o(i.ap_dcs_set_enter_sleep_mode)
    ap_dcs_set_enter_sleep_mode              0x0001207d   Thumb Code    78  s8_demo.o(i.ap_dcs_set_enter_sleep_mode)
    i.ap_dcs_set_exit_sleep_mode             0x000120d0   Section        0  s8_demo.o(i.ap_dcs_set_exit_sleep_mode)
    ap_dcs_set_exit_sleep_mode               0x000120d1   Thumb Code    36  s8_demo.o(i.ap_dcs_set_exit_sleep_mode)
    i.ap_rstn_pull_down_cb                   0x0001211c   Section        0  s8_demo.o(i.ap_rstn_pull_down_cb)
    ap_rstn_pull_down_cb                     0x0001211d   Thumb Code    38  s8_demo.o(i.ap_rstn_pull_down_cb)
    i.ap_rstn_pull_high_cb                   0x00012178   Section        0  s8_demo.o(i.ap_rstn_pull_high_cb)
    ap_rstn_pull_high_cb                     0x00012179   Thumb Code    38  s8_demo.o(i.ap_rstn_pull_high_cb)
    i.ap_set_framerate                       0x000121cc   Section        0  s8_demo.o(i.ap_set_framerate)
    ap_set_framerate                         0x000121cd   Thumb Code    20  s8_demo.o(i.ap_set_framerate)
    i.ap_update_pps_9E                       0x000121e4   Section        0  s8_demo.o(i.ap_update_pps_9E)
    ap_update_pps_9E                         0x000121e5   Thumb Code   122  s8_demo.o(i.ap_update_pps_9E)
    i.app_display_init                       0x00012268   Section        0  s8_demo.o(i.app_display_init)
    i.app_gpio_init                          0x00012294   Section        0  s8_demo.o(i.app_gpio_init)
    i.app_init_panel                         0x000122b4   Section        0  s8_demo.o(i.app_init_panel)
    app_init_panel                           0x000122b5   Thumb Code    60  s8_demo.o(i.app_init_panel)
    i.app_mipi_rx_init                       0x000122f8   Section        0  s8_demo.o(i.app_mipi_rx_init)
    app_mipi_rx_init                         0x000122f9   Thumb Code   212  s8_demo.o(i.app_mipi_rx_init)
    i.app_mipi_tx_init                       0x000123e0   Section        0  s8_demo.o(i.app_mipi_tx_init)
    app_mipi_tx_init                         0x000123e1   Thumb Code   188  s8_demo.o(i.app_mipi_tx_init)
    i.app_mipi_tx_start                      0x000124a0   Section        0  s8_demo.o(i.app_mipi_tx_start)
    app_mipi_tx_start                        0x000124a1   Thumb Code    62  s8_demo.o(i.app_mipi_tx_start)
    i.app_set_dcs_hw_ack                     0x0001250c   Section        0  s8_demo.o(i.app_set_dcs_hw_ack)
    app_set_dcs_hw_ack                       0x0001250d   Thumb Code   134  s8_demo.o(i.app_set_dcs_hw_ack)
    i.app_system_process                     0x00012598   Section        0  s8_demo.o(i.app_system_process)
    app_system_process                       0x00012599   Thumb Code    44  s8_demo.o(i.app_system_process)
    i.app_system_resume                      0x000125cc   Section        0  s8_demo.o(i.app_system_resume)
    app_system_resume                        0x000125cd   Thumb Code    30  s8_demo.o(i.app_system_resume)
    i.app_system_suspend                     0x00012614   Section        0  s8_demo.o(i.app_system_suspend)
    app_system_suspend                       0x00012615   Thumb Code   174  s8_demo.o(i.app_system_suspend)
    i.app_tx_panel_reset                     0x00012740   Section        0  s8_demo.o(i.app_tx_panel_reset)
    app_tx_panel_reset                       0x00012741   Thumb Code    46  s8_demo.o(i.app_tx_panel_reset)
    i.board_Init                             0x00012770   Section        0  board.o(i.board_Init)
    i.ceil                                   0x00012790   Section        0  ceil.o(i.ceil)
    i.check_mipi_rx_tx_video_info            0x00012858   Section        0  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    check_mipi_rx_tx_video_info              0x00012859   Thumb Code    44  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    i.check_pkt_buf_rev                      0x00012884   Section        0  hal_internal_dcs.o(i.check_pkt_buf_rev)
    check_pkt_buf_rev                        0x00012885   Thumb Code    84  hal_internal_dcs.o(i.check_pkt_buf_rev)
    i.dcs_packet_fifo_alloc                  0x0001290c   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    i.dcs_packet_fifo_init                   0x00012964   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    i.dcs_packet_free_fifo_header            0x0001297c   Section        0  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    i.dcs_packet_get_fifo_header             0x000129c0   Section        0  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    i.delayMs                                0x000129e4   Section        0  tau_delay.o(i.delayMs)
    i.delayUs                                0x000129fc   Section        0  tau_delay.o(i.delayUs)
    i.drv_common_enable_systick              0x00012a28   Section        0  drv_common.o(i.drv_common_enable_systick)
    i.drv_common_get_tick                    0x00012a80   Section        0  drv_common.o(i.drv_common_get_tick)
    i.drv_common_system_init                 0x00012a8c   Section        0  drv_common.o(i.drv_common_system_init)
    i.drv_crgu_enable_clock                  0x00012a94   Section        0  drv_crgu.o(i.drv_crgu_enable_clock)
    i.drv_crgu_get_rxbr_clk                  0x00012ad0   Section        0  drv_crgu.o(i.drv_crgu_get_rxbr_clk)
    i.drv_crgu_reset_modules                 0x00012b38   Section        0  drv_crgu.o(i.drv_crgu_reset_modules)
    i.drv_crgu_set_ahb_clk                   0x00012b48   Section        0  drv_crgu.o(i.drv_crgu_set_ahb_clk)
    i.drv_crgu_set_clock_div                 0x00012b70   Section        0  drv_crgu.o(i.drv_crgu_set_clock_div)
    i.drv_crgu_set_dpi_clk                   0x00012b80   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_clk)
    i.drv_crgu_set_dsc_clk                   0x00012bbc   Section        0  drv_crgu.o(i.drv_crgu_set_dsc_clk)
    i.drv_crgu_set_fb_clk                    0x00012bf4   Section        0  drv_crgu.o(i.drv_crgu_set_fb_clk)
    i.drv_crgu_set_lcdc_clk                  0x00012c1c   Section        0  drv_crgu.o(i.drv_crgu_set_lcdc_clk)
    i.drv_crgu_set_reset                     0x00012c44   Section        0  drv_crgu.o(i.drv_crgu_set_reset)
    i.drv_crgu_set_rxbr_clk                  0x00012c5c   Section        0  drv_crgu.o(i.drv_crgu_set_rxbr_clk)
    i.drv_crgu_set_vidc_clk                  0x00012c84   Section        0  drv_crgu.o(i.drv_crgu_set_vidc_clk)
    i.drv_dma_clear_status                   0x00012cac   Section        0  drv_dma.o(i.drv_dma_clear_status)
    i.drv_dma_get_int_source                 0x00012cc4   Section        0  drv_dma.o(i.drv_dma_get_int_source)
    drv_dma_get_int_source                   0x00012cc5   Thumb Code    16  drv_dma.o(i.drv_dma_get_int_source)
    i.drv_dsc_dec_disable                    0x00012cd8   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    i.drv_dsc_dec_enable                     0x00012cf4   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    i.drv_dsc_dec_get_nslc                   0x00012d2c   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    i.drv_dsc_dec_set_irqen                  0x00012d4c   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_set_irqen)
    i.drv_dsi_rx_calc_ipi_tx_delay           0x00012d68   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    i.drv_dsi_rx_enable_irq                  0x00012e74   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    i.drv_dsi_rx_get_color_bpp               0x00012eb4   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    drv_dsi_rx_get_color_bpp                 0x00012eb5   Thumb Code    62  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    i.drv_dsi_rx_get_color_pcc               0x00012f04   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    drv_dsi_rx_get_color_pcc                 0x00012f05   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    i.drv_dsi_rx_get_compression_en          0x00012f20   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    i.drv_dsi_rx_get_ddi_crc_en              0x00012f30   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_ddi_crc_en)
    i.drv_dsi_rx_power_up                    0x00012f40   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    i.drv_dsi_rx_set_check_crc               0x00012f58   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc)
    i.drv_dsi_rx_set_ctrl_cfg                0x00012f74   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    i.drv_dsi_rx_set_ddi_cfg                 0x00012f98   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    i.drv_dsi_rx_set_ddi_crc_en              0x00012fa8   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_crc_en)
    i.drv_dsi_rx_set_inten                   0x00012fc4   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    i.drv_dsi_rx_set_ipi_cfg                 0x00012fd0   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    i.drv_dsi_rx_set_ipi_ycbcr_frmt          0x00012fe0   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_ycbcr_frmt)
    i.drv_dsi_rx_set_lane_swap               0x00012ffc   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    i.drv_dsi_rx_set_resp_cnt                0x00013010   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    i.drv_dsi_rx_set_tear_resp_en            0x00013034   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_tear_resp_en)
    i.drv_dsi_rx_set_up_phy                  0x00013050   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    i.drv_dsi_rx_shut_down                   0x00013150   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    i.drv_dsi_tx_command_header              0x00013168   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    i.drv_dsi_tx_command_mode_cfg            0x00013180   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    i.drv_dsi_tx_command_put_payload         0x000131d8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    i.drv_dsi_tx_config_eotp                 0x000131e4   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    i.drv_dsi_tx_config_int                  0x00013204   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    i.drv_dsi_tx_dpi_lpcmd_time              0x00013210   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    i.drv_dsi_tx_dpi_mode                    0x00013220   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    i.drv_dsi_tx_dpi_polarity                0x00013230   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    i.drv_dsi_tx_edpi_cmd_size               0x00013254   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    i.drv_dsi_tx_get_cmd_status              0x00013260   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    i.drv_dsi_tx_mode                        0x0001326c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    i.drv_dsi_tx_phy_clock_lane_auto_lp      0x00013278   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    i.drv_dsi_tx_phy_clock_lane_req_hs       0x00013294   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    i.drv_dsi_tx_phy_lane_mode               0x000132b4   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    i.drv_dsi_tx_phy_status_ready            0x000132c4   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    i.drv_dsi_tx_phy_status_stopstate        0x0001332c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    i.drv_dsi_tx_phy_test_setup              0x00013370   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    i.drv_dsi_tx_phy_time_cfg                0x000134c0   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    i.drv_dsi_tx_powerup                     0x000134e0   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    i.drv_dsi_tx_response_mode               0x000134ec   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    i.drv_dsi_tx_set_bta_ack                 0x00013510   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    i.drv_dsi_tx_set_esc_div                 0x0001352c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    i.drv_dsi_tx_set_int                     0x00013540   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    i.drv_dsi_tx_set_time_out_div            0x00013580   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    i.drv_dsi_tx_set_video_chunk             0x00013598   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    i.drv_dsi_tx_set_video_timing            0x000135ac   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    i.drv_dsi_tx_shutdown                    0x000135d0   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    i.drv_dsi_tx_timeout_cfg                 0x000135dc   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    i.drv_dsi_tx_video_mode_cfg              0x00013608   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    i.drv_efuse_enter_inactive               0x000136f0   Section        0  drv_efuse.o(i.drv_efuse_enter_inactive)
    i.drv_efuse_int_enable                   0x00013726   Section        0  drv_efuse.o(i.drv_efuse_int_enable)
    i.drv_efuse_read                         0x00013732   Section        0  drv_efuse.o(i.drv_efuse_read)
    i.drv_efuse_read_req                     0x0001376c   Section        0  drv_efuse.o(i.drv_efuse_read_req)
    i.drv_gpio_get_attribute                 0x00013784   Section        0  drv_gpio.o(i.drv_gpio_get_attribute)
    i.drv_gpio_get_input_data                0x00013794   Section        0  drv_gpio.o(i.drv_gpio_get_input_data)
    i.drv_gpio_handle_int                    0x000137ac   Section        0  drv_gpio.o(i.drv_gpio_handle_int)
    drv_gpio_handle_int                      0x000137ad   Thumb Code    30  drv_gpio.o(i.drv_gpio_handle_int)
    i.drv_gpio_register_ap_reset_callback    0x000137d0   Section        0  drv_gpio.o(i.drv_gpio_register_ap_reset_callback)
    i.drv_gpio_register_callback             0x000137dc   Section        0  drv_gpio.o(i.drv_gpio_register_callback)
    i.drv_gpio_set_attribute                 0x000137f0   Section        0  drv_gpio.o(i.drv_gpio_set_attribute)
    i.drv_gpio_set_int                       0x0001380c   Section        0  drv_gpio.o(i.drv_gpio_set_int)
    i.drv_gpio_set_ioe                       0x00013850   Section        0  drv_gpio.o(i.drv_gpio_set_ioe)
    i.drv_gpio_set_mode                      0x00013870   Section        0  drv_gpio.o(i.drv_gpio_set_mode)
    i.drv_gpio_set_output_data               0x00013884   Section        0  hal_gpio.o(i.drv_gpio_set_output_data)
    drv_gpio_set_output_data                 0x00013885   Thumb Code    26  hal_gpio.o(i.drv_gpio_set_output_data)
    i.drv_lcdc_bcsa_config                   0x000138a4   Section        0  drv_lcdc.o(i.drv_lcdc_bcsa_config)
    i.drv_lcdc_cfg_int_frame                 0x000138cc   Section        0  drv_lcdc.o(i.drv_lcdc_cfg_int_frame)
    i.drv_lcdc_clear_int                     0x000138f8   Section        0  drv_lcdc.o(i.drv_lcdc_clear_int)
    drv_lcdc_clear_int                       0x000138f9   Thumb Code    20  drv_lcdc.o(i.drv_lcdc_clear_int)
    i.drv_lcdc_cmd_start                     0x00013910   Section        0  drv_lcdc.o(i.drv_lcdc_cmd_start)
    i.drv_lcdc_config_acc_command_mode       0x00013944   Section        0  drv_lcdc.o(i.drv_lcdc_config_acc_command_mode)
    i.drv_lcdc_config_int                    0x00013958   Section        0  drv_lcdc.o(i.drv_lcdc_config_int)
    i.drv_lcdc_config_int_single             0x00013990   Section        0  drv_lcdc.o(i.drv_lcdc_config_int_single)
    i.drv_lcdc_config_overwrite_rgb          0x000139b8   Section        0  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    i.drv_lcdc_config_src_parameter          0x000139d0   Section        0  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    i.drv_lcdc_crop_hact                     0x00013a20   Section        0  drv_lcdc.o(i.drv_lcdc_crop_hact)
    i.drv_lcdc_ctrl_flow                     0x00013a30   Section        0  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    i.drv_lcdc_dith_config                   0x00013a68   Section        0  drv_lcdc.o(i.drv_lcdc_dith_config)
    i.drv_lcdc_edge_dect_config              0x00013a98   Section        0  drv_lcdc.o(i.drv_lcdc_edge_dect_config)
    i.drv_lcdc_edge_enh_config               0x00013ad4   Section        0  drv_lcdc.o(i.drv_lcdc_edge_enh_config)
    i.drv_lcdc_enable_shadow_reg             0x00013b38   Section        0  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    i.drv_lcdc_endianness_config             0x00013b5c   Section        0  drv_lcdc.o(i.drv_lcdc_endianness_config)
    i.drv_lcdc_fc_config                     0x00013b78   Section        0  drv_lcdc.o(i.drv_lcdc_fc_config)
    i.drv_lcdc_fldc_config                   0x00013b98   Section        0  drv_lcdc.o(i.drv_lcdc_fldc_config)
    i.drv_lcdc_function_disable              0x00013bbc   Section        0  drv_lcdc.o(i.drv_lcdc_function_disable)
    i.drv_lcdc_function_enable               0x00013be0   Section        0  drv_lcdc.o(i.drv_lcdc_function_enable)
    i.drv_lcdc_set_int                       0x00013c04   Section        0  drv_lcdc.o(i.drv_lcdc_set_int)
    i.drv_lcdc_set_prefetch                  0x00013c40   Section        0  drv_lcdc.o(i.drv_lcdc_set_prefetch)
    i.drv_lcdc_set_tear_line                 0x00013c5c   Section        0  drv_lcdc.o(i.drv_lcdc_set_tear_line)
    i.drv_lcdc_stop_display                  0x00013c78   Section        0  drv_lcdc.o(i.drv_lcdc_stop_display)
    i.drv_lcdc_vid_hw_start                  0x00013c88   Section        0  drv_lcdc.o(i.drv_lcdc_vid_hw_start)
    i.drv_lcdc_vintp_mode_config             0x00013cc4   Section        0  drv_lcdc.o(i.drv_lcdc_vintp_mode_config)
    i.drv_memc_clear_status                  0x00013cdc   Section        0  drv_memc.o(i.drv_memc_clear_status)
    i.drv_memc_enable_irq                    0x00013cf0   Section        0  drv_memc.o(i.drv_memc_enable_irq)
    i.drv_memc_gen_a_tear_signal             0x00013d30   Section        0  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    i.drv_memc_get_status                    0x00013d40   Section        0  drv_memc.o(i.drv_memc_get_status)
    i.drv_memc_get_tear_mode                 0x00013d58   Section        0  drv_memc.o(i.drv_memc_get_tear_mode)
    i.drv_memc_rate_transfer_sel             0x00013d68   Section        0  drv_memc.o(i.drv_memc_rate_transfer_sel)
    i.drv_memc_sel_vsync                     0x00013d84   Section        0  drv_memc.o(i.drv_memc_sel_vsync)
    i.drv_memc_set_active_height             0x00013d98   Section        0  drv_memc.o(i.drv_memc_set_active_height)
    i.drv_memc_set_circ_mode_enable          0x00013db0   Section        0  drv_memc.o(i.drv_memc_set_circ_mode_enable)
    i.drv_memc_set_data_mode                 0x00013dcc   Section        0  drv_memc.o(i.drv_memc_set_data_mode)
    i.drv_memc_set_double_buffer             0x00013de0   Section        0  drv_memc.o(i.drv_memc_set_double_buffer)
    i.drv_memc_set_frame_drop_select         0x00013df8   Section        0  drv_memc.o(i.drv_memc_set_frame_drop_select)
    i.drv_memc_set_fs_en_conditions          0x00013e14   Section        0  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    i.drv_memc_set_lcdc_st_conditions        0x00013e2c   Section        0  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    i.drv_memc_set_ltpo_mode                 0x00013e48   Section        0  drv_memc.o(i.drv_memc_set_ltpo_mode)
    i.drv_memc_set_ltpo_pu_thres             0x00013e68   Section        0  drv_memc.o(i.drv_memc_set_ltpo_pu_thres)
    i.drv_memc_set_tear_mode                 0x00013e80   Section        0  drv_memc.o(i.drv_memc_set_tear_mode)
    i.drv_memc_set_tear_waveform             0x00013e94   Section        0  drv_memc.o(i.drv_memc_set_tear_waveform)
    i.drv_memc_set_vidc_sync_cnt             0x00013ec0   Section        0  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    i.drv_phy_test_clear                     0x00013ed4   Section        0  drv_phy_common.o(i.drv_phy_test_clear)
    i.drv_phy_test_lock                      0x00013ee4   Section        0  drv_phy_common.o(i.drv_phy_test_lock)
    i.drv_pwr_efuse_pd                       0x00013efc   Section        0  drv_pwr.o(i.drv_pwr_efuse_pd)
    i.drv_pwr_enter_deep_sleep_mode          0x00013f2c   Section        0  drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode)
    i.drv_pwr_enter_sleep_mode_ex            0x00013f78   Section        0  drv_pwr.o(i.drv_pwr_enter_sleep_mode_ex)
    i.drv_pwr_enter_stop_sleep_mode          0x00013fac   Section        0  drv_pwr.o(i.drv_pwr_enter_stop_sleep_mode)
    i.drv_pwr_exit_sleep_mode                0x00014044   Section        0  drv_pwr.o(i.drv_pwr_exit_sleep_mode)
    i.drv_pwr_get_power_ready_st             0x0001406c   Section        0  drv_pwr.o(i.drv_pwr_get_power_ready_st)
    i.drv_pwr_set_breath_screen_power_sel    0x0001407c   Section        0  drv_pwr.o(i.drv_pwr_set_breath_screen_power_sel)
    i.drv_pwr_set_digit_power_sel            0x000140a4   Section        0  drv_pwr.o(i.drv_pwr_set_digit_power_sel)
    i.drv_pwr_set_pll_clk                    0x000140cc   Section        0  drv_pwr.o(i.drv_pwr_set_pll_clk)
    i.drv_pwr_set_pvd                        0x00014100   Section        0  drv_pwr.o(i.drv_pwr_set_pvd)
    i.drv_pwr_set_wakeup_type                0x00014134   Section        0  drv_pwr.o(i.drv_pwr_set_wakeup_type)
    i.drv_pwr_write_lock                     0x00014160   Section        0  drv_pwr.o(i.drv_pwr_write_lock)
    i.drv_rxbr_clear_pkt_buffer              0x00014180   Section        0  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    i.drv_rxbr_clear_status0                 0x00014190   Section        0  drv_rxbr.o(i.drv_rxbr_clear_status0)
    i.drv_rxbr_enable_irq                    0x0001419c   Section        0  drv_rxbr.o(i.drv_rxbr_enable_irq)
    i.drv_rxbr_frame_drop_cfg                0x000141f8   Section        0  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    i.drv_rxbr_get_int_source                0x00014214   Section        0  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    drv_rxbr_get_int_source                  0x00014215   Thumb Code    20  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    i.drv_rxbr_get_status0                   0x0001422c   Section        0  hal_internal_dcs.o(i.drv_rxbr_get_status0)
    drv_rxbr_get_status0                     0x0001422d   Thumb Code    20  hal_internal_dcs.o(i.drv_rxbr_get_status0)
    i.drv_rxbr_hline_rcv1_cfg                0x00014244   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg)
    i.drv_rxbr_hline_rcv_cfg                 0x00014258   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    i.drv_rxbr_register_irq1_callback        0x00014268   Section        0  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    i.drv_rxbr_set_cmd_response              0x00014274   Section        0  drv_rxbr.o(i.drv_rxbr_set_cmd_response)
    i.drv_rxbr_set_color_format              0x000143b8   Section        0  drv_rxbr.o(i.drv_rxbr_set_color_format)
    i.drv_rxbr_set_filter_regs               0x000143d4   Section        0  drv_rxbr.o(i.drv_rxbr_set_filter_regs)
    i.drv_rxbr_set_inten                     0x000143f8   Section        0  drv_rxbr.o(i.drv_rxbr_set_inten)
    i.drv_rxbr_set_ltpo_drop_th              0x00014414   Section        0  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    i.drv_rxbr_set_usr_cfg                   0x0001442c   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    i.drv_rxbr_set_usr_col                   0x0001446c   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    i.drv_rxbr_set_usr_row                   0x0001447c   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    i.drv_se_init                            0x0001448c   Section        0  drv_se.o(i.drv_se_init)
    i.drv_se_set_dsc                         0x00014504   Section        0  drv_se.o(i.drv_se_set_dsc)
    i.drv_se_set_lcdc                        0x000145d8   Section        0  drv_se.o(i.drv_se_set_lcdc)
    i.drv_se_set_memc                        0x00014660   Section        0  drv_se.o(i.drv_se_set_memc)
    i.drv_se_set_rxbr                        0x000146f0   Section        0  drv_se.o(i.drv_se_set_rxbr)
    i.drv_se_set_vidc                        0x000147c0   Section        0  drv_se.o(i.drv_se_set_vidc)
    i.drv_se_start_rx                        0x0001486c   Section        0  drv_se.o(i.drv_se_start_rx)
    i.drv_spim_clear_int_status              0x00014880   Section        0  drv_spi_master.o(i.drv_spim_clear_int_status)
    i.drv_spim_disable_int                   0x0001488c   Section        0  drv_spi_master.o(i.drv_spim_disable_int)
    i.drv_spim_set_inten                     0x000148bc   Section        0  drv_spi_master.o(i.drv_spim_set_inten)
    i.drv_swire_enable                       0x000148d8   Section        0  drv_swire.o(i.drv_swire_enable)
    i.drv_swire_get_pulse_count              0x000148f4   Section        0  drv_swire.o(i.drv_swire_get_pulse_count)
    i.drv_swire_register_callback            0x00014900   Section        0  drv_swire.o(i.drv_swire_register_callback)
    i.drv_swire_set_bit_time                 0x0001490c   Section        0  drv_swire.o(i.drv_swire_set_bit_time)
    i.drv_swire_set_int                      0x00014924   Section        0  drv_swire.o(i.drv_swire_set_int)
    i.drv_swire_set_power_down               0x0001496c   Section        0  drv_swire.o(i.drv_swire_set_power_down)
    i.drv_swire_set_pulse_count              0x00014988   Section        0  drv_swire.o(i.drv_swire_set_pulse_count)
    i.drv_swire_set_trig_mode                0x00014994   Section        0  drv_swire.o(i.drv_swire_set_trig_mode)
    i.drv_sys_cfg_clear_all_int              0x000149b0   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    i.drv_sys_cfg_clear_pending              0x000149bc   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    i.drv_sys_cfg_sel_ap_rst_trig            0x000149e4   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig)
    i.drv_sys_cfg_sel_gpio_group             0x00014a08   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group)
    i.drv_sys_cfg_sel_int_trig               0x00014a2c   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig)
    i.drv_sys_cfg_sel_swire_timer            0x00014a50   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_swire_timer)
    i.drv_sys_cfg_set_int                    0x00014a68   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    i.drv_timer_clear_status_flags           0x00014a8c   Section        0  drv_timer.o(i.drv_timer_clear_status_flags)
    drv_timer_clear_status_flags             0x00014a8d   Thumb Code    26  drv_timer.o(i.drv_timer_clear_status_flags)
    i.drv_timer_enable                       0x00014aa6   Section        0  drv_timer.o(i.drv_timer_enable)
    i.drv_timer_get_instance                 0x00014ac8   Section        0  drv_timer.o(i.drv_timer_get_instance)
    i.drv_timer_handle_interrupt             0x00014ad8   Section        0  drv_timer.o(i.drv_timer_handle_interrupt)
    drv_timer_handle_interrupt               0x00014ad9   Thumb Code    54  drv_timer.o(i.drv_timer_handle_interrupt)
    i.drv_timer_set_compare_val              0x00014b14   Section        0  drv_timer.o(i.drv_timer_set_compare_val)
    i.drv_timer_set_int                      0x00014b54   Section        0  drv_timer.o(i.drv_timer_set_int)
    i.drv_timer_set_prescaler                0x00014b9c   Section        0  drv_timer.o(i.drv_timer_set_prescaler)
    i.drv_timer_set_repeat                   0x00014bc4   Section        0  drv_timer.o(i.drv_timer_set_repeat)
    i.drv_tx_phy_test_enter                  0x00014bd4   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    i.drv_tx_phy_test_exit                   0x00014bf4   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    i.drv_tx_phy_test_write_code             0x00014c14   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    i.drv_uart_abort_recv                    0x00014c3c   Section        0  drv_uart.o(i.drv_uart_abort_recv)
    i.drv_uart_abort_send                    0x00014c70   Section        0  drv_uart.o(i.drv_uart_abort_send)
    i.drv_uart_config_int                    0x00014ca4   Section        0  drv_uart.o(i.drv_uart_config_int)
    i.drv_uart_enable_clk                    0x00014cb8   Section        0  drv_uart.o(i.drv_uart_enable_clk)
    drv_uart_enable_clk                      0x00014cb9   Thumb Code    24  drv_uart.o(i.drv_uart_enable_clk)
    i.drv_uart_enable_int                    0x00014cd0   Section        0  drv_uart.o(i.drv_uart_enable_int)
    i.drv_uart_get_instance                  0x00014d2c   Section        0  drv_uart.o(i.drv_uart_get_instance)
    i.drv_uart_init                          0x00014d54   Section        0  drv_uart.o(i.drv_uart_init)
    i.drv_uart_int_trans_handle              0x00014e24   Section        0  drv_uart.o(i.drv_uart_int_trans_handle)
    drv_uart_int_trans_handle                0x00014e25   Thumb Code    54  drv_uart.o(i.drv_uart_int_trans_handle)
    i.drv_uart_reset_rx_fifo                 0x00014e60   Section        0  drv_uart.o(i.drv_uart_reset_rx_fifo)
    i.drv_uart_reset_tx_fifo                 0x00014e7c   Section        0  drv_uart.o(i.drv_uart_reset_tx_fifo)
    i.drv_uart_send_blocking                 0x00014e98   Section        0  drv_uart.o(i.drv_uart_send_blocking)
    i.drv_uart_set_baud_rate                 0x00014eb2   Section        0  drv_uart.o(i.drv_uart_set_baud_rate)
    i.drv_uart_trans_create_handle           0x00014f08   Section        0  drv_uart.o(i.drv_uart_trans_create_handle)
    i.drv_vidc_clear_irq                     0x00014f54   Section        0  drv_vidc.o(i.drv_vidc_clear_irq)
    i.drv_vidc_enable                        0x00014f64   Section        0  drv_vidc.o(i.drv_vidc_enable)
    i.drv_vidc_enable_irq                    0x00014f84   Section        0  drv_vidc.o(i.drv_vidc_enable_irq)
    i.drv_vidc_get_int_source                0x00014fc4   Section        0  drv_vidc.o(i.drv_vidc_get_int_source)
    i.drv_vidc_get_irq_status                0x00014ff0   Section        0  drv_vidc.o(i.drv_vidc_get_irq_status)
    i.drv_vidc_init_module_enable            0x00015008   Section        0  drv_vidc.o(i.drv_vidc_init_module_enable)
    i.drv_vidc_register_callback             0x00015034   Section        0  drv_vidc.o(i.drv_vidc_register_callback)
    i.drv_vidc_reset                         0x00015040   Section        0  drv_vidc.o(i.drv_vidc_reset)
    i.drv_vidc_set_circ_mode_enable          0x0001504c   Section        0  drv_vidc.o(i.drv_vidc_set_circ_mode_enable)
    i.drv_vidc_set_dither_config             0x00015068   Section        0  drv_vidc.o(i.drv_vidc_set_dither_config)
    i.drv_vidc_set_dst_parameter             0x000150a0   Section        0  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    i.drv_vidc_set_honly_hcoef0              0x000150fc   Section        0  drv_vidc.o(i.drv_vidc_set_honly_hcoef0)
    i.drv_vidc_set_honly_hinitb              0x00015108   Section        0  drv_vidc.o(i.drv_vidc_set_honly_hinitb)
    i.drv_vidc_set_honly_hinitr              0x00015134   Section        0  drv_vidc.o(i.drv_vidc_set_honly_hinitr)
    i.drv_vidc_set_irqen                     0x00015164   Section        0  drv_vidc.o(i.drv_vidc_set_irqen)
    i.drv_vidc_set_mirror                    0x00015180   Section        0  drv_vidc.o(i.drv_vidc_set_mirror)
    i.drv_vidc_set_pentile_swap              0x00015194   Section        0  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    i.drv_vidc_set_pu_ctrl                   0x000151b0   Section        0  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    i.drv_vidc_set_rotation                  0x000151bc   Section        0  drv_vidc.o(i.drv_vidc_set_rotation)
    i.drv_vidc_set_scld_hcoef0               0x000151d4   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    i.drv_vidc_set_scld_hcoef1               0x000151e0   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    i.drv_vidc_set_scld_step                 0x000151ec   Section        0  drv_vidc.o(i.drv_vidc_set_scld_step)
    i.drv_vidc_set_scld_vcoef0               0x00015200   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    i.drv_vidc_set_scld_vcoef1               0x0001520c   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    i.drv_vidc_set_src_parameter             0x00015218   Section        0  drv_vidc.o(i.drv_vidc_set_src_parameter)
    i.drv_vidc_set_vintp_config              0x00015238   Section        0  drv_vidc.o(i.drv_vidc_set_vintp_config)
    i.fputc                                  0x00015270   Section        0  tau_log.o(i.fputc)
    i.ha_intl_fb_check_pu_size               0x000152a4   Section        0  hal_internal_fb.o(i.ha_intl_fb_check_pu_size)
    ha_intl_fb_check_pu_size                 0x000152a5   Thumb Code    58  hal_internal_fb.o(i.ha_intl_fb_check_pu_size)
    i.hal_dsi_rx_ctrl_create_handle          0x000152e4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    i.hal_dsi_rx_ctrl_dcs_async_handler      0x00015324   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler)
    i.hal_dsi_rx_ctrl_deinit                 0x00015364   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit)
    i.hal_dsi_rx_ctrl_init                   0x000153f8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    i.hal_dsi_rx_ctrl_init_clk               0x000154a4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    hal_dsi_rx_ctrl_init_clk                 0x000154a5   Thumb Code   222  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    i.hal_dsi_rx_ctrl_init_dsi_rx            0x000155a4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    hal_dsi_rx_ctrl_init_dsi_rx              0x000155a5   Thumb Code   232  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    i.hal_dsi_rx_ctrl_init_memc              0x000156ac   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    hal_dsi_rx_ctrl_init_memc                0x000156ad   Thumb Code   294  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    i.hal_dsi_rx_ctrl_init_rxbr              0x000157d8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    hal_dsi_rx_ctrl_init_rxbr                0x000157d9   Thumb Code   314  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    i.hal_dsi_rx_ctrl_init_vidc              0x00015920   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    hal_dsi_rx_ctrl_init_vidc                0x00015921   Thumb Code   624  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    i.hal_dsi_rx_ctrl_pre_init_pps           0x00015ba0   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    i.hal_dsi_rx_ctrl_set_auto_ack           0x00015bd8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack)
    i.hal_dsi_rx_ctrl_set_ipi_cfg            0x00015c88   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    hal_dsi_rx_ctrl_set_ipi_cfg              0x00015c89   Thumb Code    48  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    i.hal_dsi_rx_ctrl_start                  0x00015cb8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    i.hal_dsi_rx_ctrl_stop                   0x00015ce8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop)
    i.hal_dsi_rx_ctrl_toggle_resolution      0x00015d18   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    i.hal_dsi_tx_cmd_mode_cal_timing         0x00015d38   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing)
    hal_dsi_tx_cmd_mode_cal_timing           0x00015d39   Thumb Code   506  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing)
    i.hal_dsi_tx_ctrl_create_handle          0x00015fb4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    i.hal_dsi_tx_ctrl_deinit                 0x00015fec   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit)
    i.hal_dsi_tx_ctrl_gen_a_tear_signal      0x00016060   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal)
    i.hal_dsi_tx_ctrl_init                   0x00016084   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    i.hal_dsi_tx_ctrl_init_clk               0x00016100   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    hal_dsi_tx_ctrl_init_clk                 0x00016101   Thumb Code    12  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    i.hal_dsi_tx_ctrl_set_overwrite_rgb      0x00016110   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    i.hal_dsi_tx_ctrl_set_tear_mode          0x00016118   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode)
    i.hal_dsi_tx_ctrl_start                  0x00016124   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    i.hal_dsi_tx_ctrl_stop                   0x000161b4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop)
    i.hal_dsi_tx_ctrl_write_array_cmd        0x000161ec   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd)
    i.hal_dsi_tx_ctrl_write_cmd              0x000162e0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    i.hal_dsi_tx_init_cfg                    0x000163b0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg)
    hal_dsi_tx_init_cfg                      0x000163b1   Thumb Code   250  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg)
    i.hal_dsi_tx_init_dpi_timing             0x000164b4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing)
    hal_dsi_tx_init_dpi_timing               0x000164b5   Thumb Code    58  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing)
    i.hal_dsi_tx_init_phy_cfg                0x000164f8   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    hal_dsi_tx_init_phy_cfg                  0x000164f9   Thumb Code    22  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    i.hal_dsi_tx_init_timing                 0x0001650e   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing)
    hal_dsi_tx_init_timing                   0x0001650f   Thumb Code    82  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing)
    i.hal_dsi_tx_init_vid_timing             0x00016560   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing)
    hal_dsi_tx_init_vid_timing               0x00016561   Thumb Code    70  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing)
    i.hal_dsi_tx_send_cmd                    0x000165b4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    hal_dsi_tx_send_cmd                      0x000165b5   Thumb Code    58  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    i.hal_dsi_tx_timing_info_update          0x000165f4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update)
    hal_dsi_tx_timing_info_update            0x000165f5   Thumb Code   142  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update)
    i.hal_dsi_tx_vid_mode_cal_timing         0x00016688   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing)
    hal_dsi_tx_vid_mode_cal_timing           0x00016689   Thumb Code   766  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing)
    i.hal_gpio_config_pad                    0x00016998   Section        0  hal_gpio.o(i.hal_gpio_config_pad)
    i.hal_gpio_ctrl_eint                     0x000169d4   Section        0  hal_gpio.o(i.hal_gpio_ctrl_eint)
    i.hal_gpio_get_input_data                0x000169ec   Section        0  hal_gpio.o(i.hal_gpio_get_input_data)
    i.hal_gpio_init_eint                     0x00016a00   Section        0  hal_gpio.o(i.hal_gpio_init_eint)
    i.hal_gpio_init_input                    0x00016a40   Section        0  hal_gpio.o(i.hal_gpio_init_input)
    i.hal_gpio_init_output                   0x00016a56   Section        0  hal_gpio.o(i.hal_gpio_init_output)
    i.hal_gpio_reg_eint_cb                   0x00016a74   Section        0  hal_gpio.o(i.hal_gpio_reg_eint_cb)
    i.hal_gpio_set_ap_reset_int              0x00016a90   Section        0  hal_gpio.o(i.hal_gpio_set_ap_reset_int)
    i.hal_gpio_set_mode                      0x00016ae0   Section        0  hal_gpio.o(i.hal_gpio_set_mode)
    i.hal_gpio_set_output_data               0x00016b40   Section        0  hal_gpio.o(i.hal_gpio_set_output_data)
    i.hal_gpio_set_pull_state                0x00016b48   Section        0  hal_gpio.o(i.hal_gpio_set_pull_state)
    i.hal_internal_sync_get_hight_performan_mode 0x00016b90   Section        0  hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode)
    i.hal_internal_sync_input_resolution_change 0x00016ba0   Section        0  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    i.hal_internal_sync_register_lcdc_cb     0x00016d54   Section        0  hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb)
    i.hal_internal_vsync_deinit              0x00016d60   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    i.hal_internal_vsync_get_rx_state        0x00016d80   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state)
    i.hal_internal_vsync_get_sync_line       0x00016d8c   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    i.hal_internal_vsync_get_tx_state        0x00016da0   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    i.hal_internal_vsync_init_rx             0x00016dac   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    i.hal_internal_vsync_init_tx             0x00016e94   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    i.hal_internal_vsync_set_rx_state        0x00016f5c   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    i.hal_internal_vsync_set_tear_mode       0x00016f7c   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    i.hal_internal_vsync_set_tx_state        0x000170b8   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    i.hal_intl_dcs_init_sw_fltr              0x00017110   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr)
    i.hal_intl_dcs_rx_get_dcs_packet_data    0x0001717c   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data)
    hal_intl_dcs_rx_get_dcs_packet_data      0x0001717d   Thumb Code   806  hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data)
    i.hal_intl_dcs_rx_receive_packet         0x000175c8   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet)
    hal_intl_dcs_rx_receive_packet           0x000175c9   Thumb Code   122  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet)
    i.hal_intl_dcs_rx_receive_pps            0x00017650   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps)
    hal_intl_dcs_rx_receive_pps              0x00017651   Thumb Code   266  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps)
    i.hal_intl_dcs_set_auto_hw_filter        0x000177c4   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter)
    i.hal_intl_dcs_sw_filter_handle          0x00017850   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle)
    hal_intl_dcs_sw_filter_handle            0x00017851   Thumb Code    36  hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle)
    i.hal_intl_fb_cal_fb_info                0x0001787c   Section        0  hal_internal_fb.o(i.hal_intl_fb_cal_fb_info)
    i.hal_intl_fb_check_bandwidth            0x00017b6c   Section        0  hal_internal_fb.o(i.hal_intl_fb_check_bandwidth)
    hal_intl_fb_check_bandwidth              0x00017b6d   Thumb Code    92  hal_internal_fb.o(i.hal_intl_fb_check_bandwidth)
    i.hal_intl_fb_edge_resize                0x00017bd0   Section        0  hal_internal_fb.o(i.hal_intl_fb_edge_resize)
    hal_intl_fb_edge_resize                  0x00017bd1   Thumb Code   214  hal_internal_fb.o(i.hal_intl_fb_edge_resize)
    i.hal_intl_fb_flow_control_adapter       0x00017cac   Section        0  hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter)
    hal_intl_fb_flow_control_adapter         0x00017cad   Thumb Code   110  hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter)
    i.hal_intl_fb_get_memc_flow_mode         0x00017d20   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode)
    i.hal_intl_fb_get_rx_fb_info             0x00017d2c   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info)
    i.hal_intl_fb_get_tx_fb_info             0x00017d3c   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info)
    i.hal_intl_fb_get_user_flow              0x00017d4c   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_user_flow)
    i.hal_intl_svs_deinit_rx                 0x00017d58   Section        0  hal_internal_svs.o(i.hal_intl_svs_deinit_rx)
    i.hal_intl_svs_deinit_tx                 0x00017d80   Section        0  hal_internal_svs.o(i.hal_intl_svs_deinit_tx)
    i.hal_intl_svs_handle                    0x00017d90   Section        0  hal_internal_svs.o(i.hal_intl_svs_handle)
    i.hal_intl_svs_init_rx                   0x00017db4   Section        0  hal_internal_svs.o(i.hal_intl_svs_init_rx)
    i.hal_intl_svs_init_tx                   0x00017e34   Section        0  hal_internal_svs.o(i.hal_intl_svs_init_tx)
    i.hal_intl_svs_set_rx_vtt                0x00017e48   Section        0  hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt)
    i.hal_intl_svs_update_rxbr_clk           0x00017e54   Section        0  hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk)
    i.hal_lcdc_displayproc_config            0x00017e9c   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config)
    i.hal_lcdc_init_cfg                      0x00017f0c   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    hal_lcdc_init_cfg                        0x00017f0d   Thumb Code    62  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    i.hal_lcdc_init_clk                      0x00017f4a   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    hal_lcdc_init_clk                        0x00017f4b   Thumb Code   112  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    i.hal_lcdc_postproc_config               0x00017fbc   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config)
    i.hal_lcdc_start                         0x000180e4   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_start)
    hal_lcdc_start                           0x000180e5   Thumb Code    36  hal_dsi_tx_ctrl.o(i.hal_lcdc_start)
    i.hal_lcdc_timinggen_config              0x00018108   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config)
    hal_lcdc_timinggen_config                0x00018109   Thumb Code    60  hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config)
    i.hal_lcdc_upscaler_config               0x00018144   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config)
    i.hal_nonshadow_func_update              0x00018224   Section        0  hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update)
    i.hal_pwr_enter_deep_sleep_mode          0x000182e0   Section        0  hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode)
    i.hal_pwr_enter_normal_sleep_mode        0x0001830a   Section        0  hal_pwr.o(i.hal_pwr_enter_normal_sleep_mode)
    i.hal_pwr_enter_stop_sleep_mode          0x00018314   Section        0  hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode)
    i.hal_pwr_exit_sleep_mode                0x00018378   Section        0  hal_pwr.o(i.hal_pwr_exit_sleep_mode)
    i.hal_pwr_get_vcc_power_ready            0x00018382   Section        0  hal_pwr.o(i.hal_pwr_get_vcc_power_ready)
    i.hal_pwr_set_main_power                 0x0001838a   Section        0  hal_pwr.o(i.hal_pwr_set_main_power)
    i.hal_pwr_set_pvd                        0x00018392   Section        0  hal_pwr.o(i.hal_pwr_set_pvd)
    i.hal_pwr_set_sleep_mode_power           0x0001839a   Section        0  hal_pwr.o(i.hal_pwr_set_sleep_mode_power)
    i.hal_pwr_set_stop_sleep_wakeup_pin      0x000183a4   Section        0  hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin)
    i.hal_swire_deinit                       0x00018408   Section        0  hal_swire.o(i.hal_swire_deinit)
    i.hal_swire_enable                       0x00018448   Section        0  hal_swire.o(i.hal_swire_enable)
    i.hal_swire_init                         0x000184a4   Section        0  hal_swire.o(i.hal_swire_init)
    i.hal_swire_set_pulse                    0x000184fc   Section        0  hal_swire.o(i.hal_swire_set_pulse)
    i.hal_swire_set_timer                    0x00018520   Section        0  hal_swire.o(i.hal_swire_set_timer)
    i.hal_system_enable_systick              0x00018560   Section        0  hal_system.o(i.hal_system_enable_systick)
    i.hal_system_get_tick                    0x00018568   Section        0  hal_system.o(i.hal_system_get_tick)
    i.hal_system_init                        0x00018570   Section        0  hal_system.o(i.hal_system_init)
    i.hal_system_updata_sysclk               0x00018654   Section        0  hal_system.o(i.hal_system_updata_sysclk)
    i.hal_timer_deinit                       0x000186a4   Section        0  hal_timer.o(i.hal_timer_deinit)
    i.hal_timer_init                         0x000186d4   Section        0  hal_timer.o(i.hal_timer_init)
    i.hal_timer_set_repeat                   0x000186f0   Section        0  hal_timer.o(i.hal_timer_set_repeat)
    i.hal_tx_frame_rate_adjust               0x000186f8   Section        0  hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust)
    hal_tx_frame_rate_adjust                 0x000186f9   Thumb Code    44  hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust)
    i.hal_uart_init                          0x00018728   Section        0  hal_uart.o(i.hal_uart_init)
    i.hal_uart_send_blocking                 0x000187bc   Section        0  hal_uart.o(i.hal_uart_send_blocking)
    i.hal_vsync_func_update                  0x000187d8   Section        0  hal_dsi_tx_ctrl.o(i.hal_vsync_func_update)
    i.hal_vsync_reset_lcdc_scaler            0x000187f0   Section        0  hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler)
    i.main                                   0x000188d0   Section        0  main.o(i.main)
    i.pps_update_handle                      0x00018910   Section        0  s8_demo.o(i.pps_update_handle)
    pps_update_handle                        0x00018911   Thumb Code    76  s8_demo.o(i.pps_update_handle)
    i.rxbr_irq1_callback                     0x00018964   Section        0  hal_internal_vsync.o(i.rxbr_irq1_callback)
    rxbr_irq1_callback                       0x00018965   Thumb Code   478  hal_internal_vsync.o(i.rxbr_irq1_callback)
    i.s8_demo                                0x00018c48   Section        0  s8_demo.o(i.s8_demo)
    i.send_panel_init_code                   0x00018cac   Section        0  s8_demo.o(i.send_panel_init_code)
    send_panel_init_code                     0x00018cad   Thumb Code    58  s8_demo.o(i.send_panel_init_code)
    i.soft_double_buffer_update              0x00018ce8   Section        0  hal_internal_vsync.o(i.soft_double_buffer_update)
    soft_double_buffer_update                0x00018ce9   Thumb Code    56  hal_internal_vsync.o(i.soft_double_buffer_update)
    i.soft_gen_te                            0x00018d2c   Section        0  hal_internal_vsync.o(i.soft_gen_te)
    soft_gen_te                              0x00018d2d   Thumb Code    86  hal_internal_vsync.o(i.soft_gen_te)
    i.soft_gen_te_double_buffer              0x00018d98   Section        0  hal_internal_vsync.o(i.soft_gen_te_double_buffer)
    soft_gen_te_double_buffer                0x00018d99   Thumb Code   202  hal_internal_vsync.o(i.soft_gen_te_double_buffer)
    i.soft_pro_motion_init                   0x00018e78   Section        0  hal_internal_vsync.o(i.soft_pro_motion_init)
    soft_pro_motion_init                     0x00018e79   Thumb Code    46  hal_internal_vsync.o(i.soft_pro_motion_init)
    i.soft_tear_adjust_line                  0x00018eb0   Section        0  hal_internal_vsync.o(i.soft_tear_adjust_line)
    soft_tear_adjust_line                    0x00018eb1   Thumb Code    26  hal_internal_vsync.o(i.soft_tear_adjust_line)
    i.stop_sleep_cb                          0x00018ed4   Section        0  hal_pwr.o(i.stop_sleep_cb)
    stop_sleep_cb                            0x00018ed5   Thumb Code    18  hal_pwr.o(i.stop_sleep_cb)
    i.svs_direct_mode_setting                0x00018eec   Section        0  hal_internal_svs.o(i.svs_direct_mode_setting)
    svs_direct_mode_setting                  0x00018eed   Thumb Code   154  hal_internal_svs.o(i.svs_direct_mode_setting)
    i.svs_get_rel_intv                       0x00018f98   Section        0  hal_internal_svs.o(i.svs_get_rel_intv)
    svs_get_rel_intv                         0x00018f99   Thumb Code    20  hal_internal_svs.o(i.svs_get_rel_intv)
    i.svs_sync_handle                        0x00018fb4   Section        0  hal_internal_svs.o(i.svs_sync_handle)
    svs_sync_handle                          0x00018fb5   Thumb Code   158  hal_internal_svs.o(i.svs_sync_handle)
    i.svs_wait_fr_stab                       0x00019064   Section        0  hal_internal_svs.o(i.svs_wait_fr_stab)
    svs_wait_fr_stab                         0x00019065   Thumb Code   148  hal_internal_svs.o(i.svs_wait_fr_stab)
    i.svs_wait_start                         0x00019130   Section        0  hal_internal_svs.o(i.svs_wait_start)
    svs_wait_start                           0x00019131   Thumb Code   250  hal_internal_svs.o(i.svs_wait_start)
    i.tau_log_init                           0x0001923c   Section        0  tau_log.o(i.tau_log_init)
    i.tau_log_printf                         0x00019270   Section        0  tau_log.o(i.tau_log_printf)
    i.tau_log_push_log                       0x000192f4   Section        0  tau_log.o(i.tau_log_push_log)
    i.vidc_callback                          0x0001936c   Section        0  hal_internal_vsync.o(i.vidc_callback)
    vidc_callback                            0x0001936d   Thumb Code   150  hal_internal_vsync.o(i.vidc_callback)
    i.vpre_err_reset                         0x00019420   Section        0  hal_internal_vsync.o(i.vpre_err_reset)
    vpre_err_reset                           0x00019421   Thumb Code   254  hal_internal_vsync.o(i.vpre_err_reset)
    .constdata                               0x00019538   Section     7944  s8_demo.o(.constdata)
    g_cus_rx_dcs_execute_table               0x00019538   Data         108  s8_demo.o(.constdata)
    .constdata                               0x0001b440   Section       40  hal_dsi_rx_ctrl.o(.constdata)
    .constdata                               0x0001b468   Section       28  hal_dsi_tx_ctrl.o(.constdata)
    .constdata                               0x0001b484   Section      182  hal_gpio.o(.constdata)
    s_gpio_map                               0x0001b484   Data         104  hal_gpio.o(.constdata)
    s_gpio_perf                              0x0001b4ec   Data          78  hal_gpio.o(.constdata)
    .constdata                               0x0001b53c   Section       48  hal_uart.o(.constdata)
    .constdata                               0x0001b56c   Section       16  drv_uart.o(.constdata)
    .conststring                             0x0001b57c   Section      135  hal_dsi_rx_ctrl.o(.conststring)
    .conststring                             0x0001b604   Section      144  hal_internal_vsync.o(.conststring)
    .conststring                             0x0001b694   Section      142  hal_internal_dcs.o(.conststring)
    .data                                    0x00070000   Section      148  s8_demo.o(.data)
    g_rx_ctrl_handle                         0x00070000   Data           4  s8_demo.o(.data)
    g_tx_ctrl_handle                         0x00070004   Data           4  s8_demo.o(.data)
    panel_display_done                       0x00070008   Data           1  s8_demo.o(.data)
    sg_system_resume                         0x00070009   Data           1  s8_demo.o(.data)
    sg_system_suspend                        0x0007000a   Data           1  s8_demo.o(.data)
    AP_REG51_7FF                             0x0007000b   Data           1  s8_demo.o(.data)
    sg_aod_in_flag                           0x0007000c   Data           1  s8_demo.o(.data)
    Flag                                     0x0007008e   Data           1  s8_demo.o(.data)
    ExitDelay                                0x00070090   Data           4  s8_demo.o(.data)
    .data                                    0x00070094   Section       36  hal_dsi_rx_ctrl.o(.data)
    g_hw_auto_filter                         0x00070094   Data           1  hal_dsi_rx_ctrl.o(.data)
    g_crc_check_enable                       0x00070095   Data           1  hal_dsi_rx_ctrl.o(.data)
    g_esc_clk                                0x00070098   Data           4  hal_dsi_rx_ctrl.o(.data)
    g_before_draw_col                        0x0007009c   Data           4  hal_dsi_rx_ctrl.o(.data)
    g_before_draw_page                       0x000700a0   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_step                                 0x000700a4   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_cmd_filter                           0x000700a8   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_x                                    0x000700ac   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_y                                    0x000700b0   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_value                                0x000700b4   Data           4  hal_dsi_rx_ctrl.o(.data)
    .data                                    0x000700b8   Section       92  hal_dsi_tx_ctrl.o(.data)
    sg_bta_vsync_flag                        0x000700b8   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_vsync_flag                            0x000700b9   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_enter_sleep_cmd                       0x000700ba   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_fldc_cg_mode                          0x000700bb   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_scl_fir                        0x000700bc   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_honly_bypass_fir                      0x000700bd   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_bcs                            0x000700be   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_enhc                           0x000700bf   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_edge_dect                      0x000700c0   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_edge_enh                       0x000700c1   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_dith                           0x000700c2   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_dith_judge                            0x000700c3   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_endianness                            0x000700c4   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_test_pattern_en                       0x000700c5   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_dith_judge_thr                        0x000700c8   Data           4  hal_dsi_tx_ctrl.o(.data)
    sg_ccm_para                              0x000700cc   Data          36  hal_dsi_tx_ctrl.o(.data)
    sg_honly_para                            0x000700f0   Data          36  hal_dsi_tx_ctrl.o(.data)
    .data                                    0x00070114   Section        1  hal_spi_master.o(.data)
    sg_spim_trans_end                        0x00070114   Data           1  hal_spi_master.o(.data)
    .data                                    0x00070115   Section        2  hal_swire.o(.data)
    sg_swire_timer                           0x00070115   Data           1  hal_swire.o(.data)
    sg_swire_repeat                          0x00070116   Data           1  hal_swire.o(.data)
    .data                                    0x00070118   Section        8  hal_pwr.o(.data)
    sg_wake_up_io                            0x00070118   Data           1  hal_pwr.o(.data)
    sg_stop_sleep_wakeup_int                 0x0007011c   Data           4  hal_pwr.o(.data)
    .data                                    0x00070120   Section        1  tau_log.o(.data)
    g_log_port                               0x00070120   Data           1  tau_log.o(.data)
    .data                                    0x00070124   Section       24  hal_uart.o(.data)
    sg_dma_callback                          0x00070134   Data           4  hal_uart.o(.data)
    sg_user_data                             0x00070138   Data           4  hal_uart.o(.data)
    .data                                    0x0007013c   Section       16  hal_internal_vsync.o(.data)
    s_te_refine_mode                         0x0007013c   Data           1  hal_internal_vsync.o(.data)
    .data                                    0x0007014c   Section       36  hal_internal_dcs.o(.data)
    g_imm_packet                             0x0007014c   Data          24  hal_internal_dcs.o(.data)
    g_cus_rx_write_cmd_handle                0x00070164   Data          12  hal_internal_dcs.o(.data)
    .data                                    0x00070170   Section       12  drv_common.o(.data)
    s_my_tick                                0x00070170   Data           4  drv_common.o(.data)
    .data                                    0x0007017c   Section        1  drv_common.o(.data)
    .data                                    0x00070180   Section      400  drv_dma.o(.data)
    sg_dma_handle                            0x00070180   Data         256  drv_dma.o(.data)
    .data                                    0x00070310   Section        4  drv_gpio.o(.data)
    g_ap_reset_cb                            0x00070310   Data           4  drv_gpio.o(.data)
    .data                                    0x00070314   Section        4  drv_swire.o(.data)
    sg_drv_swire_cb                          0x00070314   Data           4  drv_swire.o(.data)
    .data                                    0x00070318   Section       80  drv_timer.o(.data)
    sg_timer_info                            0x00070318   Data          80  drv_timer.o(.data)
    .data                                    0x00070368   Section       36  drv_i2c.o(.data)
    .data                                    0x0007038c   Section        4  drv_se.o(.data)
    chip_info                                0x0007038c   Data           4  drv_se.o(.data)
    .data                                    0x00070390   Section        1  drv_dsi_rx.o(.data)
    sg_rx_drv_level                          0x00070390   Data           1  drv_dsi_rx.o(.data)
    .data                                    0x00070394   Section        8  drv_rxbr.o(.data)
    .data                                    0x0007039c   Section        4  drv_vidc.o(.data)
    .data                                    0x000703a0   Section        4  stdout.o(.data)
    .bss                                     0x000703a4   Section      208  hal_dsi_rx_ctrl.o(.bss)
    g_rx_ctrl_handle                         0x000703a4   Data         208  hal_dsi_rx_ctrl.o(.bss)
    .bss                                     0x00070474   Section      184  hal_dsi_tx_ctrl.o(.bss)
    g_tx_ctrl_handle                         0x00070474   Data          92  hal_dsi_tx_ctrl.o(.bss)
    sg_dsi_tx_param                          0x000704d0   Data          92  hal_dsi_tx_ctrl.o(.bss)
    .bss                                     0x0007052c   Section      256  tau_log.o(.bss)
    g_log_buf                                0x0007052c   Data         256  tau_log.o(.bss)
    .bss                                     0x0007062c   Section       68  hal_internal_vsync.o(.bss)
    .bss                                     0x00070670   Section     2048  hal_internal_dcs.o(.bss)
    .bss                                     0x00070e70   Section      255  hal_internal_dcs.o(.bss)
    g_imm_buffer                             0x00070e70   Data         255  hal_internal_dcs.o(.bss)
    .bss                                     0x00070f70   Section       68  hal_internal_fb.o(.bss)
    .bss                                     0x00070fb4   Section       68  hal_internal_svs.o(.bss)
    sg_sys_handler                           0x00070fb4   Data          68  hal_internal_svs.o(.bss)
    .bss                                     0x00070ff8   Section       16  drv_dma.o(.bss)
    sg_dma_int_list                          0x00070ff8   Data          16  drv_dma.o(.bss)
    .bss                                     0x00071008   Section       64  drv_gpio.o(.bss)
    s_gpio_cb                                0x00071008   Data          64  drv_gpio.o(.bss)
    .bss                                     0x00071048   Section     4204  dcs_packet_fifo.o(.bss)
    .bss                                     0x000720b4   Section       96  drv_uart.o(.bss)
    sg_uart_userdata                         0x000720b4   Data          96  drv_uart.o(.bss)
    STACK                                    0x00072118   Section     4096  startup_armcm0.o(STACK)

    Global Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    BuildAttributes$$THM_ISAv3M$S$PE$A:L22$X:L11$S22$IEEE1$IW$USESV6$~STKCKD$USESV7$~SHL$OTIME$ROPI$IEEEJ$EBA8$MICROLIB$REQ8$PRES8$EABIv2 0x00000000   Number         0  anon$$obj.o ABSOLUTE
    __ARM_use_no_argv                        0x00000000   Number         0  main.o ABSOLUTE
    _printf_a                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_c                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_charcount                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_d                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_e                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_f                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_flags                            0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_dec                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_hex                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_g                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_i                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_int_dec                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_l                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ll                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lld                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lli                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llo                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llu                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llx                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_dec                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_hex                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_oct                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ls                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_mbtowc                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_n                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_o                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_p                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_percent                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_pre_padding                      0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_return_value                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_s                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_sizespec                         0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_str                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_signed                  0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_unsigned                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_u                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wctomb                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_widthprec                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_x                                0x00000000   Number         0  stubs.o ABSOLUTE
    __cpp_initialize__aeabi_                  - Undefined Weak Reference
    __cxa_finalize                            - Undefined Weak Reference
    _clock_init                               - Undefined Weak Reference
    _microlib_exit                            - Undefined Weak Reference
    __Vectors_Size                           0x000000c0   Number         0  startup_armcm0.o ABSOLUTE
    __Vectors                                0x00010000   Data           4  startup_armcm0.o(RESET)
    __Vectors_End                            0x000100c0   Data           0  startup_armcm0.o(RESET)
    __main                                   0x000100c1   Thumb Code     0  entry.o(.ARM.Collect$$$$00000000)
    _main_stk                                0x000100c1   Thumb Code     0  entry2.o(.ARM.Collect$$$$00000001)
    _main_scatterload                        0x000100c5   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    __main_after_scatterload                 0x000100c9   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    _main_clock                              0x000100c9   Thumb Code     0  entry7b.o(.ARM.Collect$$$$00000008)
    _main_cpp_init                           0x000100c9   Thumb Code     0  entry8b.o(.ARM.Collect$$$$0000000A)
    _main_init                               0x000100c9   Thumb Code     0  entry9a.o(.ARM.Collect$$$$0000000B)
    __rt_final_cpp                           0x000100d1   Thumb Code     0  entry10a.o(.ARM.Collect$$$$0000000D)
    __rt_final_exit                          0x000100d1   Thumb Code     0  entry11a.o(.ARM.Collect$$$$0000000F)
    Reset_Handler                            0x000100d5   Thumb Code    28  startup_armcm0.o(.text)
    NMI_Handler                              0x000100f1   Thumb Code     2  startup_armcm0.o(.text)
    SVC_Handler                              0x000100f5   Thumb Code     2  startup_armcm0.o(.text)
    PendSV_Handler                           0x000100f7   Thumb Code     2  startup_armcm0.o(.text)
    FLSCTRL_IRQn_Handler                     0x00010107   Thumb Code     2  startup_armcm0.o(.text)
    WDG_IRQn_Handler                         0x00010113   Thumb Code     2  startup_armcm0.o(.text)
    SPIS_IRQn_Handler                        0x0001011b   Thumb Code     2  startup_armcm0.o(.text)
    OTP_IRQn_Handler                         0x00010123   Thumb Code     2  startup_armcm0.o(.text)
    PVD_IRQn_Handler                         0x00010127   Thumb Code     2  startup_armcm0.o(.text)
    __aeabi_uidiv                            0x0001014d   Thumb Code     0  uidiv.o(.text)
    __aeabi_uidivmod                         0x0001014d   Thumb Code    44  uidiv.o(.text)
    __aeabi_idiv                             0x00010179   Thumb Code     0  idiv.o(.text)
    __aeabi_idivmod                          0x00010179   Thumb Code    40  idiv.o(.text)
    __aeabi_memcpy                           0x000101a1   Thumb Code    36  memcpya.o(.text)
    __aeabi_memcpy4                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memcpy8                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memset                           0x000101c5   Thumb Code    14  memseta.o(.text)
    __aeabi_memset4                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memset8                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr                           0x000101d3   Thumb Code     4  memseta.o(.text)
    __aeabi_memclr4                          0x000101d3   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr8                          0x000101d3   Thumb Code     0  memseta.o(.text)
    _memset$wrapper                          0x000101d7   Thumb Code    18  memseta.o(.text)
    strlen                                   0x000101e9   Thumb Code    14  strlen.o(.text)
    memcmp                                   0x000101f7   Thumb Code    26  memcmp.o(.text)
    __aeabi_fadd                             0x00010211   Thumb Code   162  fadd.o(.text)
    __aeabi_fsub                             0x000102b3   Thumb Code     8  fadd.o(.text)
    __aeabi_frsub                            0x000102bb   Thumb Code     8  fadd.o(.text)
    __aeabi_fmul                             0x000102c3   Thumb Code   122  fmul.o(.text)
    __aeabi_fdiv                             0x0001033d   Thumb Code   124  fdiv.o(.text)
    __ARM_scalbnf                            0x000103b9   Thumb Code    24  fscalb.o(.text)
    scalbnf                                  0x000103b9   Thumb Code     0  fscalb.o(.text)
    __aeabi_dadd                             0x000103d1   Thumb Code   328  dadd.o(.text)
    __aeabi_dsub                             0x00010519   Thumb Code    12  dadd.o(.text)
    __aeabi_drsub                            0x00010525   Thumb Code    12  dadd.o(.text)
    __aeabi_dmul                             0x00010535   Thumb Code   202  dmul.o(.text)
    __aeabi_ddiv                             0x00010605   Thumb Code   234  ddiv.o(.text)
    __aeabi_ui2f                             0x000106f5   Thumb Code    14  ffltui.o(.text)
    __aeabi_ui2d                             0x00010705   Thumb Code    24  dfltui.o(.text)
    __aeabi_f2uiz                            0x00010721   Thumb Code    40  ffixui.o(.text)
    __aeabi_d2uiz                            0x00010749   Thumb Code    50  dfixui.o(.text)
    __aeabi_f2d                              0x00010785   Thumb Code    40  f2d.o(.text)
    __aeabi_d2f                              0x000107ad   Thumb Code    56  d2f.o(.text)
    __aeabi_cfcmpeq                          0x000107e5   Thumb Code     0  cfcmple.o(.text)
    __aeabi_cfcmple                          0x000107e5   Thumb Code    20  cfcmple.o(.text)
    __aeabi_cfrcmple                         0x000107f9   Thumb Code    20  cfrcmple.o(.text)
    __aeabi_uldivmod                         0x0001080d   Thumb Code    96  uldiv.o(.text)
    __aeabi_llsl                             0x0001086d   Thumb Code    32  llshl.o(.text)
    _ll_shift_l                              0x0001086d   Thumb Code     0  llshl.o(.text)
    __aeabi_llsr                             0x0001088d   Thumb Code    34  llushr.o(.text)
    _ll_ushift_r                             0x0001088d   Thumb Code     0  llushr.o(.text)
    __aeabi_lasr                             0x000108af   Thumb Code    38  llsshr.o(.text)
    _ll_sshift_r                             0x000108af   Thumb Code     0  llsshr.o(.text)
    __I$use$fp                               0x000108d5   Thumb Code     0  iusefp.o(.text)
    _float_round                             0x000108d5   Thumb Code    16  fepilogue.o(.text)
    _float_epilogue                          0x000108e5   Thumb Code   114  fepilogue.o(.text)
    _double_round                            0x00010957   Thumb Code    26  depilogue.o(.text)
    _double_epilogue                         0x00010971   Thumb Code   164  depilogue.o(.text)
    __aeabi_d2ulz                            0x00010a15   Thumb Code    54  dfixul.o(.text)
    __aeabi_cdrcmple                         0x00010a55   Thumb Code    38  cdrcmple.o(.text)
    __scatterload                            0x00010a7d   Thumb Code    28  init.o(.text)
    __scatterload_rt2                        0x00010a7d   Thumb Code     0  init.o(.text)
    __decompress                             0x00010aa1   Thumb Code     0  __dczerorl2.o(.text)
    __decompress1                            0x00010aa1   Thumb Code    86  __dczerorl2.o(.text)
    AP_NRESET_IRQn_Handler                   0x00010af9   Thumb Code    22  drv_gpio.o(i.AP_NRESET_IRQn_Handler)
    DMA_IRQn_Handler                         0x00010b15   Thumb Code    78  drv_dma.o(i.DMA_IRQn_Handler)
    EXTI_INT0_IRQn_Handler                   0x00010b71   Thumb Code    10  drv_gpio.o(i.EXTI_INT0_IRQn_Handler)
    EXTI_INT1_IRQn_Handler                   0x00010b7b   Thumb Code    10  drv_gpio.o(i.EXTI_INT1_IRQn_Handler)
    EXTI_INT2_IRQn_Handler                   0x00010b85   Thumb Code    10  drv_gpio.o(i.EXTI_INT2_IRQn_Handler)
    EXTI_INT3_IRQn_Handler                   0x00010b8f   Thumb Code    10  drv_gpio.o(i.EXTI_INT3_IRQn_Handler)
    EXTI_INT4_IRQn_Handler                   0x00010b99   Thumb Code    10  drv_gpio.o(i.EXTI_INT4_IRQn_Handler)
    EXTI_INT5_IRQn_Handler                   0x00010ba3   Thumb Code    10  drv_gpio.o(i.EXTI_INT5_IRQn_Handler)
    EXTI_INT6_IRQn_Handler                   0x00010bad   Thumb Code    10  drv_gpio.o(i.EXTI_INT6_IRQn_Handler)
    EXTI_INT7_IRQn_Handler                   0x00010bb7   Thumb Code    10  drv_gpio.o(i.EXTI_INT7_IRQn_Handler)
    HardFault_Handler                        0x00010bc1   Thumb Code    14  drv_common.o(i.HardFault_Handler)
    I2C0_IRQn_Handler                        0x00010c09   Thumb Code     8  drv_i2c.o(i.I2C0_IRQn_Handler)
    I2C1_IRQn_Handler                        0x00010c15   Thumb Code     8  drv_i2c.o(i.I2C1_IRQn_Handler)
    I2C2_IRQn_Handler                        0x00010c21   Thumb Code     8  drv_i2c.o(i.I2C2_IRQn_Handler)
    LCDC_IRQn_Handler                        0x00010c2d   Thumb Code   118  hal_internal_vsync.o(i.LCDC_IRQn_Handler)
    MEMC_IRQn_Handler                        0x00010d2d   Thumb Code   154  drv_memc.o(i.MEMC_IRQn_Handler)
    MIPI_TX_IRQn_Handler                     0x00010dc9   Thumb Code    70  drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler)
    SPIM_IRQn_Handler                        0x00010f35   Thumb Code    62  hal_spi_master.o(i.SPIM_IRQn_Handler)
    SWIRE_IRQn_Handler                       0x00010f7d   Thumb Code    38  drv_swire.o(i.SWIRE_IRQn_Handler)
    SysTick_Handler                          0x00010fad   Thumb Code    20  drv_common.o(i.SysTick_Handler)
    TIMER0_IRQn_Handler                      0x00010fc5   Thumb Code    10  drv_timer.o(i.TIMER0_IRQn_Handler)
    TIMER1_IRQn_Handler                      0x00010fcf   Thumb Code    10  drv_timer.o(i.TIMER1_IRQn_Handler)
    TIMER2_IRQn_Handler                      0x00010fd9   Thumb Code    10  drv_timer.o(i.TIMER2_IRQn_Handler)
    TIMER3_IRQn_Handler                      0x00010fe3   Thumb Code    10  drv_timer.o(i.TIMER3_IRQn_Handler)
    __scatterload_copy                       0x00010fed   Thumb Code    14  handlers.o(i.__scatterload_copy)
    __scatterload_null                       0x00010ffb   Thumb Code     2  handlers.o(i.__scatterload_null)
    s_RAM_CK                                 0x00011000   Data          28  drv_common.o(.ARM.__at_0x11000)
    g_tau_log                                0x0001101c   Data          16  tau_log.o(.ARM.__at_0x1101C)
    sg_pq_para                               0x0001102c   Data          22  hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C)
    MIPI_RX_IRQn_Handler                     0x00011045   Thumb Code   354  drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler)
    UART_IRQn_Handler                        0x000113a9   Thumb Code   364  drv_uart.o(i.UART_IRQn_Handler)
    VIDC_IRQn_Handler                        0x00011529   Thumb Code    22  drv_vidc.o(i.VIDC_IRQn_Handler)
    VPRE1_IRQn_Handler                       0x00011545   Thumb Code    22  drv_rxbr.o(i.VPRE1_IRQn_Handler)
    VPRE_IRQn_Handler                        0x00011561   Thumb Code   104  hal_internal_dcs.o(i.VPRE_IRQn_Handler)
    __0printf                                0x000115cd   Thumb Code    24  printfa.o(i.__0printf)
    __1printf                                0x000115cd   Thumb Code     0  printfa.o(i.__0printf)
    __2printf                                0x000115cd   Thumb Code     0  printfa.o(i.__0printf)
    __c89printf                              0x000115cd   Thumb Code     0  printfa.o(i.__0printf)
    printf                                   0x000115cd   Thumb Code     0  printfa.o(i.__0printf)
    __0vsprintf                              0x000115ed   Thumb Code    30  printfa.o(i.__0vsprintf)
    __1vsprintf                              0x000115ed   Thumb Code     0  printfa.o(i.__0vsprintf)
    __2vsprintf                              0x000115ed   Thumb Code     0  printfa.o(i.__0vsprintf)
    __c89vsprintf                            0x000115ed   Thumb Code     0  printfa.o(i.__0vsprintf)
    vsprintf                                 0x000115ed   Thumb Code     0  printfa.o(i.__0vsprintf)
    __ARM_clz                                0x00011611   Thumb Code    46  depilogue.o(i.__ARM_clz)
    __ARM_common_switch8                     0x0001163f   Thumb Code    26  hal_dsi_rx_ctrl.o(i.__ARM_common_switch8)
    __scatterload_zeroinit                   0x00011691   Thumb Code    14  handlers.o(i.__scatterload_zeroinit)
    app_display_init                         0x00012269   Thumb Code    44  s8_demo.o(i.app_display_init)
    app_gpio_init                            0x00012295   Thumb Code    28  s8_demo.o(i.app_gpio_init)
    board_Init                               0x00012771   Thumb Code    26  board.o(i.board_Init)
    ceil                                     0x00012791   Thumb Code   180  ceil.o(i.ceil)
    dcs_packet_fifo_alloc                    0x0001290d   Thumb Code    80  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    dcs_packet_fifo_init                     0x00012965   Thumb Code    18  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    dcs_packet_free_fifo_header              0x0001297d   Thumb Code    60  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    dcs_packet_get_fifo_header               0x000129c1   Thumb Code    26  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    delayMs                                  0x000129e5   Thumb Code    24  tau_delay.o(i.delayMs)
    delayUs                                  0x000129fd   Thumb Code    40  tau_delay.o(i.delayUs)
    drv_common_enable_systick                0x00012a29   Thumb Code    70  drv_common.o(i.drv_common_enable_systick)
    drv_common_get_tick                      0x00012a81   Thumb Code     6  drv_common.o(i.drv_common_get_tick)
    drv_common_system_init                   0x00012a8d   Thumb Code     8  drv_common.o(i.drv_common_system_init)
    drv_crgu_enable_clock                    0x00012a95   Thumb Code    54  drv_crgu.o(i.drv_crgu_enable_clock)
    drv_crgu_get_rxbr_clk                    0x00012ad1   Thumb Code    70  drv_crgu.o(i.drv_crgu_get_rxbr_clk)
    drv_crgu_reset_modules                   0x00012b39   Thumb Code    10  drv_crgu.o(i.drv_crgu_reset_modules)
    drv_crgu_set_ahb_clk                     0x00012b49   Thumb Code    34  drv_crgu.o(i.drv_crgu_set_ahb_clk)
    drv_crgu_set_clock_div                   0x00012b71   Thumb Code    12  drv_crgu.o(i.drv_crgu_set_clock_div)
    drv_crgu_set_dpi_clk                     0x00012b81   Thumb Code    54  drv_crgu.o(i.drv_crgu_set_dpi_clk)
    drv_crgu_set_dsc_clk                     0x00012bbd   Thumb Code    52  drv_crgu.o(i.drv_crgu_set_dsc_clk)
    drv_crgu_set_fb_clk                      0x00012bf5   Thumb Code    34  drv_crgu.o(i.drv_crgu_set_fb_clk)
    drv_crgu_set_lcdc_clk                    0x00012c1d   Thumb Code    36  drv_crgu.o(i.drv_crgu_set_lcdc_clk)
    drv_crgu_set_reset                       0x00012c45   Thumb Code    20  drv_crgu.o(i.drv_crgu_set_reset)
    drv_crgu_set_rxbr_clk                    0x00012c5d   Thumb Code    34  drv_crgu.o(i.drv_crgu_set_rxbr_clk)
    drv_crgu_set_vidc_clk                    0x00012c85   Thumb Code    36  drv_crgu.o(i.drv_crgu_set_vidc_clk)
    drv_dma_clear_status                     0x00012cad   Thumb Code    20  drv_dma.o(i.drv_dma_clear_status)
    drv_dsc_dec_disable                      0x00012cd9   Thumb Code    20  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    drv_dsc_dec_enable                       0x00012cf5   Thumb Code    44  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    drv_dsc_dec_get_nslc                     0x00012d2d   Thumb Code    22  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    drv_dsc_dec_set_irqen                    0x00012d4d   Thumb Code    24  drv_dsc_dec.o(i.drv_dsc_dec_set_irqen)
    drv_dsi_rx_calc_ipi_tx_delay             0x00012d69   Thumb Code   252  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    drv_dsi_rx_enable_irq                    0x00012e75   Thumb Code    58  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    drv_dsi_rx_get_compression_en            0x00012f21   Thumb Code    10  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    drv_dsi_rx_get_ddi_crc_en                0x00012f31   Thumb Code    10  drv_dsi_rx.o(i.drv_dsi_rx_get_ddi_crc_en)
    drv_dsi_rx_power_up                      0x00012f41   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    drv_dsi_rx_set_check_crc                 0x00012f59   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc)
    drv_dsi_rx_set_ctrl_cfg                  0x00012f75   Thumb Code    32  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    drv_dsi_rx_set_ddi_cfg                   0x00012f99   Thumb Code    10  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    drv_dsi_rx_set_ddi_crc_en                0x00012fa9   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_crc_en)
    drv_dsi_rx_set_inten                     0x00012fc5   Thumb Code     8  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    drv_dsi_rx_set_ipi_cfg                   0x00012fd1   Thumb Code    12  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    drv_dsi_rx_set_ipi_ycbcr_frmt            0x00012fe1   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_ycbcr_frmt)
    drv_dsi_rx_set_lane_swap                 0x00012ffd   Thumb Code    16  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    drv_dsi_rx_set_resp_cnt                  0x00013011   Thumb Code    32  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    drv_dsi_rx_set_tear_resp_en              0x00013035   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_tear_resp_en)
    drv_dsi_rx_set_up_phy                    0x00013051   Thumb Code   224  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    drv_dsi_rx_shut_down                     0x00013151   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    drv_dsi_tx_command_header                0x00013169   Thumb Code    18  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    drv_dsi_tx_command_mode_cfg              0x00013181   Thumb Code    82  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    drv_dsi_tx_command_put_payload           0x000131d9   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    drv_dsi_tx_config_eotp                   0x000131e5   Thumb Code    26  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    drv_dsi_tx_config_int                    0x00013205   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    drv_dsi_tx_dpi_lpcmd_time                0x00013211   Thumb Code    10  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    drv_dsi_tx_dpi_mode                      0x00013221   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    drv_dsi_tx_dpi_polarity                  0x00013231   Thumb Code    32  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    drv_dsi_tx_edpi_cmd_size                 0x00013255   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    drv_dsi_tx_get_cmd_status                0x00013261   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    drv_dsi_tx_mode                          0x0001326d   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    drv_dsi_tx_phy_clock_lane_auto_lp        0x00013279   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    drv_dsi_tx_phy_clock_lane_req_hs         0x00013295   Thumb Code    26  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    drv_dsi_tx_phy_lane_mode                 0x000132b5   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    drv_dsi_tx_phy_status_ready              0x000132c5   Thumb Code   100  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    drv_dsi_tx_phy_status_stopstate          0x0001332d   Thumb Code    62  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    drv_dsi_tx_phy_test_setup                0x00013371   Thumb Code   314  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    drv_dsi_tx_phy_time_cfg                  0x000134c1   Thumb Code    28  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    drv_dsi_tx_powerup                       0x000134e1   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    drv_dsi_tx_response_mode                 0x000134ed   Thumb Code    30  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    drv_dsi_tx_set_bta_ack                   0x00013511   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    drv_dsi_tx_set_esc_div                   0x0001352d   Thumb Code    14  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    drv_dsi_tx_set_int                       0x00013541   Thumb Code    58  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    drv_dsi_tx_set_time_out_div              0x00013581   Thumb Code    18  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    drv_dsi_tx_set_video_chunk               0x00013599   Thumb Code    14  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    drv_dsi_tx_set_video_timing              0x000135ad   Thumb Code    30  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    drv_dsi_tx_shutdown                      0x000135d1   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    drv_dsi_tx_timeout_cfg                   0x000135dd   Thumb Code    38  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    drv_dsi_tx_video_mode_cfg                0x00013609   Thumb Code   226  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    drv_efuse_enter_inactive                 0x000136f1   Thumb Code    54  drv_efuse.o(i.drv_efuse_enter_inactive)
    drv_efuse_int_enable                     0x00013727   Thumb Code    12  drv_efuse.o(i.drv_efuse_int_enable)
    drv_efuse_read                           0x00013733   Thumb Code    58  drv_efuse.o(i.drv_efuse_read)
    drv_efuse_read_req                       0x0001376d   Thumb Code    24  drv_efuse.o(i.drv_efuse_read_req)
    drv_gpio_get_attribute                   0x00013785   Thumb Code    12  drv_gpio.o(i.drv_gpio_get_attribute)
    drv_gpio_get_input_data                  0x00013795   Thumb Code    20  drv_gpio.o(i.drv_gpio_get_input_data)
    drv_gpio_register_ap_reset_callback      0x000137d1   Thumb Code     6  drv_gpio.o(i.drv_gpio_register_ap_reset_callback)
    drv_gpio_register_callback               0x000137dd   Thumb Code    14  drv_gpio.o(i.drv_gpio_register_callback)
    drv_gpio_set_attribute                   0x000137f1   Thumb Code    22  drv_gpio.o(i.drv_gpio_set_attribute)
    drv_gpio_set_int                         0x0001380d   Thumb Code    62  drv_gpio.o(i.drv_gpio_set_int)
    drv_gpio_set_ioe                         0x00013851   Thumb Code    26  drv_gpio.o(i.drv_gpio_set_ioe)
    drv_gpio_set_mode                        0x00013871   Thumb Code    16  drv_gpio.o(i.drv_gpio_set_mode)
    drv_lcdc_bcsa_config                     0x000138a5   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_bcsa_config)
    drv_lcdc_cfg_int_frame                   0x000138cd   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_cfg_int_frame)
    drv_lcdc_cmd_start                       0x00013911   Thumb Code    46  drv_lcdc.o(i.drv_lcdc_cmd_start)
    drv_lcdc_config_acc_command_mode         0x00013945   Thumb Code    14  drv_lcdc.o(i.drv_lcdc_config_acc_command_mode)
    drv_lcdc_config_int                      0x00013959   Thumb Code    50  drv_lcdc.o(i.drv_lcdc_config_int)
    drv_lcdc_config_int_single               0x00013991   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_int_single)
    drv_lcdc_config_overwrite_rgb            0x000139b9   Thumb Code    18  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    drv_lcdc_config_src_parameter            0x000139d1   Thumb Code    72  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    drv_lcdc_crop_hact                       0x00013a21   Thumb Code    10  drv_lcdc.o(i.drv_lcdc_crop_hact)
    drv_lcdc_ctrl_flow                       0x00013a31   Thumb Code    50  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    drv_lcdc_dith_config                     0x00013a69   Thumb Code    40  drv_lcdc.o(i.drv_lcdc_dith_config)
    drv_lcdc_edge_dect_config                0x00013a99   Thumb Code    50  drv_lcdc.o(i.drv_lcdc_edge_dect_config)
    drv_lcdc_edge_enh_config                 0x00013ad5   Thumb Code    86  drv_lcdc.o(i.drv_lcdc_edge_enh_config)
    drv_lcdc_enable_shadow_reg               0x00013b39   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    drv_lcdc_endianness_config               0x00013b5d   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_endianness_config)
    drv_lcdc_fc_config                       0x00013b79   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_fc_config)
    drv_lcdc_fldc_config                     0x00013b99   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_fldc_config)
    drv_lcdc_function_disable                0x00013bbd   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_function_disable)
    drv_lcdc_function_enable                 0x00013be1   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_function_enable)
    drv_lcdc_set_int                         0x00013c05   Thumb Code    54  drv_lcdc.o(i.drv_lcdc_set_int)
    drv_lcdc_set_prefetch                    0x00013c41   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_set_prefetch)
    drv_lcdc_set_tear_line                   0x00013c5d   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_set_tear_line)
    drv_lcdc_stop_display                    0x00013c79   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_stop_display)
    drv_lcdc_vid_hw_start                    0x00013c89   Thumb Code    56  drv_lcdc.o(i.drv_lcdc_vid_hw_start)
    drv_lcdc_vintp_mode_config               0x00013cc5   Thumb Code    18  drv_lcdc.o(i.drv_lcdc_vintp_mode_config)
    drv_memc_clear_status                    0x00013cdd   Thumb Code    14  drv_memc.o(i.drv_memc_clear_status)
    drv_memc_enable_irq                      0x00013cf1   Thumb Code    58  drv_memc.o(i.drv_memc_enable_irq)
    drv_memc_gen_a_tear_signal               0x00013d31   Thumb Code    12  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    drv_memc_get_status                      0x00013d41   Thumb Code    20  drv_memc.o(i.drv_memc_get_status)
    drv_memc_get_tear_mode                   0x00013d59   Thumb Code    10  drv_memc.o(i.drv_memc_get_tear_mode)
    drv_memc_rate_transfer_sel               0x00013d69   Thumb Code    22  drv_memc.o(i.drv_memc_rate_transfer_sel)
    drv_memc_sel_vsync                       0x00013d85   Thumb Code    16  drv_memc.o(i.drv_memc_sel_vsync)
    drv_memc_set_active_height               0x00013d99   Thumb Code    16  drv_memc.o(i.drv_memc_set_active_height)
    drv_memc_set_circ_mode_enable            0x00013db1   Thumb Code    24  drv_memc.o(i.drv_memc_set_circ_mode_enable)
    drv_memc_set_data_mode                   0x00013dcd   Thumb Code    14  drv_memc.o(i.drv_memc_set_data_mode)
    drv_memc_set_double_buffer               0x00013de1   Thumb Code    18  drv_memc.o(i.drv_memc_set_double_buffer)
    drv_memc_set_frame_drop_select           0x00013df9   Thumb Code    24  drv_memc.o(i.drv_memc_set_frame_drop_select)
    drv_memc_set_fs_en_conditions            0x00013e15   Thumb Code    18  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    drv_memc_set_lcdc_st_conditions          0x00013e2d   Thumb Code    20  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    drv_memc_set_ltpo_mode                   0x00013e49   Thumb Code    28  drv_memc.o(i.drv_memc_set_ltpo_mode)
    drv_memc_set_ltpo_pu_thres               0x00013e69   Thumb Code    18  drv_memc.o(i.drv_memc_set_ltpo_pu_thres)
    drv_memc_set_tear_mode                   0x00013e81   Thumb Code    16  drv_memc.o(i.drv_memc_set_tear_mode)
    drv_memc_set_tear_waveform               0x00013e95   Thumb Code    36  drv_memc.o(i.drv_memc_set_tear_waveform)
    drv_memc_set_vidc_sync_cnt               0x00013ec1   Thumb Code    16  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    drv_phy_test_clear                       0x00013ed5   Thumb Code    16  drv_phy_common.o(i.drv_phy_test_clear)
    drv_phy_test_lock                        0x00013ee5   Thumb Code    24  drv_phy_common.o(i.drv_phy_test_lock)
    drv_pwr_efuse_pd                         0x00013efd   Thumb Code    36  drv_pwr.o(i.drv_pwr_efuse_pd)
    drv_pwr_enter_deep_sleep_mode            0x00013f2d   Thumb Code    60  drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode)
    drv_pwr_enter_sleep_mode_ex              0x00013f79   Thumb Code    34  drv_pwr.o(i.drv_pwr_enter_sleep_mode_ex)
    drv_pwr_enter_stop_sleep_mode            0x00013fad   Thumb Code   132  drv_pwr.o(i.drv_pwr_enter_stop_sleep_mode)
    drv_pwr_exit_sleep_mode                  0x00014045   Thumb Code    32  drv_pwr.o(i.drv_pwr_exit_sleep_mode)
    drv_pwr_get_power_ready_st               0x0001406d   Thumb Code    10  drv_pwr.o(i.drv_pwr_get_power_ready_st)
    drv_pwr_set_breath_screen_power_sel      0x0001407d   Thumb Code    34  drv_pwr.o(i.drv_pwr_set_breath_screen_power_sel)
    drv_pwr_set_digit_power_sel              0x000140a5   Thumb Code    34  drv_pwr.o(i.drv_pwr_set_digit_power_sel)
    drv_pwr_set_pll_clk                      0x000140cd   Thumb Code    30  drv_pwr.o(i.drv_pwr_set_pll_clk)
    drv_pwr_set_pvd                          0x00014101   Thumb Code    40  drv_pwr.o(i.drv_pwr_set_pvd)
    drv_pwr_set_wakeup_type                  0x00014135   Thumb Code    40  drv_pwr.o(i.drv_pwr_set_wakeup_type)
    drv_pwr_write_lock                       0x00014161   Thumb Code    18  drv_pwr.o(i.drv_pwr_write_lock)
    drv_rxbr_clear_pkt_buffer                0x00014181   Thumb Code    12  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    drv_rxbr_clear_status0                   0x00014191   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_clear_status0)
    drv_rxbr_enable_irq                      0x0001419d   Thumb Code    90  drv_rxbr.o(i.drv_rxbr_enable_irq)
    drv_rxbr_frame_drop_cfg                  0x000141f9   Thumb Code    18  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    drv_rxbr_hline_rcv1_cfg                  0x00014245   Thumb Code    14  drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg)
    drv_rxbr_hline_rcv_cfg                   0x00014259   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    drv_rxbr_register_irq1_callback          0x00014269   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    drv_rxbr_set_cmd_response                0x00014275   Thumb Code   320  drv_rxbr.o(i.drv_rxbr_set_cmd_response)
    drv_rxbr_set_color_format                0x000143b9   Thumb Code    24  drv_rxbr.o(i.drv_rxbr_set_color_format)
    drv_rxbr_set_filter_regs                 0x000143d5   Thumb Code    32  drv_rxbr.o(i.drv_rxbr_set_filter_regs)
    drv_rxbr_set_inten                       0x000143f9   Thumb Code    22  drv_rxbr.o(i.drv_rxbr_set_inten)
    drv_rxbr_set_ltpo_drop_th                0x00014415   Thumb Code    18  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    drv_rxbr_set_usr_cfg                     0x0001442d   Thumb Code    56  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    drv_rxbr_set_usr_col                     0x0001446d   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    drv_rxbr_set_usr_row                     0x0001447d   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    drv_se_init                              0x0001448d   Thumb Code   106  drv_se.o(i.drv_se_init)
    drv_se_set_dsc                           0x00014505   Thumb Code   162  drv_se.o(i.drv_se_set_dsc)
    drv_se_set_lcdc                          0x000145d9   Thumb Code    88  drv_se.o(i.drv_se_set_lcdc)
    drv_se_set_memc                          0x00014661   Thumb Code    96  drv_se.o(i.drv_se_set_memc)
    drv_se_set_rxbr                          0x000146f1   Thumb Code   158  drv_se.o(i.drv_se_set_rxbr)
    drv_se_set_vidc                          0x000147c1   Thumb Code   122  drv_se.o(i.drv_se_set_vidc)
    drv_se_start_rx                          0x0001486d   Thumb Code    16  drv_se.o(i.drv_se_start_rx)
    drv_spim_clear_int_status                0x00014881   Thumb Code     8  drv_spi_master.o(i.drv_spim_clear_int_status)
    drv_spim_disable_int                     0x0001488d   Thumb Code    38  drv_spi_master.o(i.drv_spim_disable_int)
    drv_spim_set_inten                       0x000148bd   Thumb Code    22  drv_spi_master.o(i.drv_spim_set_inten)
    drv_swire_enable                         0x000148d9   Thumb Code    24  drv_swire.o(i.drv_swire_enable)
    drv_swire_get_pulse_count                0x000148f5   Thumb Code     6  drv_swire.o(i.drv_swire_get_pulse_count)
    drv_swire_register_callback              0x00014901   Thumb Code     6  drv_swire.o(i.drv_swire_register_callback)
    drv_swire_set_bit_time                   0x0001490d   Thumb Code    18  drv_swire.o(i.drv_swire_set_bit_time)
    drv_swire_set_int                        0x00014925   Thumb Code    64  drv_swire.o(i.drv_swire_set_int)
    drv_swire_set_power_down                 0x0001496d   Thumb Code    24  drv_swire.o(i.drv_swire_set_power_down)
    drv_swire_set_pulse_count                0x00014989   Thumb Code     6  drv_swire.o(i.drv_swire_set_pulse_count)
    drv_swire_set_trig_mode                  0x00014995   Thumb Code    24  drv_swire.o(i.drv_swire_set_trig_mode)
    drv_sys_cfg_clear_all_int                0x000149b1   Thumb Code     8  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    drv_sys_cfg_clear_pending                0x000149bd   Thumb Code    32  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    drv_sys_cfg_sel_ap_rst_trig              0x000149e5   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig)
    drv_sys_cfg_sel_gpio_group               0x00014a09   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group)
    drv_sys_cfg_sel_int_trig                 0x00014a2d   Thumb Code    32  drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig)
    drv_sys_cfg_sel_swire_timer              0x00014a51   Thumb Code    18  drv_sys_cfg.o(i.drv_sys_cfg_sel_swire_timer)
    drv_sys_cfg_set_int                      0x00014a69   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    drv_timer_enable                         0x00014aa7   Thumb Code    32  drv_timer.o(i.drv_timer_enable)
    drv_timer_get_instance                   0x00014ac9   Thumb Code    10  drv_timer.o(i.drv_timer_get_instance)
    drv_timer_set_compare_val                0x00014b15   Thumb Code    50  drv_timer.o(i.drv_timer_set_compare_val)
    drv_timer_set_int                        0x00014b55   Thumb Code    68  drv_timer.o(i.drv_timer_set_int)
    drv_timer_set_prescaler                  0x00014b9d   Thumb Code    36  drv_timer.o(i.drv_timer_set_prescaler)
    drv_timer_set_repeat                     0x00014bc5   Thumb Code    12  drv_timer.o(i.drv_timer_set_repeat)
    drv_tx_phy_test_enter                    0x00014bd5   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    drv_tx_phy_test_exit                     0x00014bf5   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    drv_tx_phy_test_write_code               0x00014c15   Thumb Code    34  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    drv_uart_abort_recv                      0x00014c3d   Thumb Code    46  drv_uart.o(i.drv_uart_abort_recv)
    drv_uart_abort_send                      0x00014c71   Thumb Code    46  drv_uart.o(i.drv_uart_abort_send)
    drv_uart_config_int                      0x00014ca5   Thumb Code    20  drv_uart.o(i.drv_uart_config_int)
    drv_uart_enable_int                      0x00014cd1   Thumb Code    84  drv_uart.o(i.drv_uart_enable_int)
    drv_uart_get_instance                    0x00014d2d   Thumb Code    36  drv_uart.o(i.drv_uart_get_instance)
    drv_uart_init                            0x00014d55   Thumb Code   206  drv_uart.o(i.drv_uart_init)
    drv_uart_reset_rx_fifo                   0x00014e61   Thumb Code    28  drv_uart.o(i.drv_uart_reset_rx_fifo)
    drv_uart_reset_tx_fifo                   0x00014e7d   Thumb Code    28  drv_uart.o(i.drv_uart_reset_tx_fifo)
    drv_uart_send_blocking                   0x00014e99   Thumb Code    26  drv_uart.o(i.drv_uart_send_blocking)
    drv_uart_set_baud_rate                   0x00014eb3   Thumb Code    84  drv_uart.o(i.drv_uart_set_baud_rate)
    drv_uart_trans_create_handle             0x00014f09   Thumb Code    72  drv_uart.o(i.drv_uart_trans_create_handle)
    drv_vidc_clear_irq                       0x00014f55   Thumb Code    10  drv_vidc.o(i.drv_vidc_clear_irq)
    drv_vidc_enable                          0x00014f65   Thumb Code    26  drv_vidc.o(i.drv_vidc_enable)
    drv_vidc_enable_irq                      0x00014f85   Thumb Code    58  drv_vidc.o(i.drv_vidc_enable_irq)
    drv_vidc_get_int_source                  0x00014fc5   Thumb Code    40  drv_vidc.o(i.drv_vidc_get_int_source)
    drv_vidc_get_irq_status                  0x00014ff1   Thumb Code    20  drv_vidc.o(i.drv_vidc_get_irq_status)
    drv_vidc_init_module_enable              0x00015009   Thumb Code    36  drv_vidc.o(i.drv_vidc_init_module_enable)
    drv_vidc_register_callback               0x00015035   Thumb Code     6  drv_vidc.o(i.drv_vidc_register_callback)
    drv_vidc_reset                           0x00015041   Thumb Code     8  drv_vidc.o(i.drv_vidc_reset)
    drv_vidc_set_circ_mode_enable            0x0001504d   Thumb Code    24  drv_vidc.o(i.drv_vidc_set_circ_mode_enable)
    drv_vidc_set_dither_config               0x00015069   Thumb Code    50  drv_vidc.o(i.drv_vidc_set_dither_config)
    drv_vidc_set_dst_parameter               0x000150a1   Thumb Code    86  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    drv_vidc_set_honly_hcoef0                0x000150fd   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_honly_hcoef0)
    drv_vidc_set_honly_hinitb                0x00015109   Thumb Code    38  drv_vidc.o(i.drv_vidc_set_honly_hinitb)
    drv_vidc_set_honly_hinitr                0x00015135   Thumb Code    42  drv_vidc.o(i.drv_vidc_set_honly_hinitr)
    drv_vidc_set_irqen                       0x00015165   Thumb Code    22  drv_vidc.o(i.drv_vidc_set_irqen)
    drv_vidc_set_mirror                      0x00015181   Thumb Code    16  drv_vidc.o(i.drv_vidc_set_mirror)
    drv_vidc_set_pentile_swap                0x00015195   Thumb Code    20  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    drv_vidc_set_pu_ctrl                     0x000151b1   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    drv_vidc_set_rotation                    0x000151bd   Thumb Code    18  drv_vidc.o(i.drv_vidc_set_rotation)
    drv_vidc_set_scld_hcoef0                 0x000151d5   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    drv_vidc_set_scld_hcoef1                 0x000151e1   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    drv_vidc_set_scld_step                   0x000151ed   Thumb Code    14  drv_vidc.o(i.drv_vidc_set_scld_step)
    drv_vidc_set_scld_vcoef0                 0x00015201   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    drv_vidc_set_scld_vcoef1                 0x0001520d   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    drv_vidc_set_src_parameter               0x00015219   Thumb Code    28  drv_vidc.o(i.drv_vidc_set_src_parameter)
    drv_vidc_set_vintp_config                0x00015239   Thumb Code    52  drv_vidc.o(i.drv_vidc_set_vintp_config)
    fputc                                    0x00015271   Thumb Code    42  tau_log.o(i.fputc)
    hal_dsi_rx_ctrl_create_handle            0x000152e5   Thumb Code    60  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    hal_dsi_rx_ctrl_dcs_async_handler        0x00015325   Thumb Code    60  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler)
    hal_dsi_rx_ctrl_deinit                   0x00015365   Thumb Code   132  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit)
    hal_dsi_rx_ctrl_init                     0x000153f9   Thumb Code   158  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    hal_dsi_rx_ctrl_pre_init_pps             0x00015ba1   Thumb Code    50  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    hal_dsi_rx_ctrl_set_auto_ack             0x00015bd9   Thumb Code   148  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack)
    hal_dsi_rx_ctrl_start                    0x00015cb9   Thumb Code    42  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    hal_dsi_rx_ctrl_stop                     0x00015ce9   Thumb Code    42  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop)
    hal_dsi_rx_ctrl_toggle_resolution        0x00015d19   Thumb Code    28  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    hal_dsi_tx_ctrl_create_handle            0x00015fb5   Thumb Code    48  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    hal_dsi_tx_ctrl_deinit                   0x00015fed   Thumb Code   102  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit)
    hal_dsi_tx_ctrl_gen_a_tear_signal        0x00016061   Thumb Code    34  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal)
    hal_dsi_tx_ctrl_init                     0x00016085   Thumb Code   110  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    hal_dsi_tx_ctrl_set_overwrite_rgb        0x00016111   Thumb Code     8  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    hal_dsi_tx_ctrl_set_tear_mode            0x00016119   Thumb Code    10  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode)
    hal_dsi_tx_ctrl_start                    0x00016125   Thumb Code   134  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    hal_dsi_tx_ctrl_stop                     0x000161b5   Thumb Code    52  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop)
    hal_dsi_tx_ctrl_write_array_cmd          0x000161ed   Thumb Code   238  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd)
    hal_dsi_tx_ctrl_write_cmd                0x000162e1   Thumb Code   202  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    hal_gpio_config_pad                      0x00016999   Thumb Code    58  hal_gpio.o(i.hal_gpio_config_pad)
    hal_gpio_ctrl_eint                       0x000169d5   Thumb Code    18  hal_gpio.o(i.hal_gpio_ctrl_eint)
    hal_gpio_get_input_data                  0x000169ed   Thumb Code    18  hal_gpio.o(i.hal_gpio_get_input_data)
    hal_gpio_init_eint                       0x00016a01   Thumb Code    58  hal_gpio.o(i.hal_gpio_init_eint)
    hal_gpio_init_input                      0x00016a41   Thumb Code    22  hal_gpio.o(i.hal_gpio_init_input)
    hal_gpio_init_output                     0x00016a57   Thumb Code    28  hal_gpio.o(i.hal_gpio_init_output)
    hal_gpio_reg_eint_cb                     0x00016a75   Thumb Code    22  hal_gpio.o(i.hal_gpio_reg_eint_cb)
    hal_gpio_set_ap_reset_int                0x00016a91   Thumb Code    76  hal_gpio.o(i.hal_gpio_set_ap_reset_int)
    hal_gpio_set_mode                        0x00016ae1   Thumb Code    92  hal_gpio.o(i.hal_gpio_set_mode)
    hal_gpio_set_output_data                 0x00016b41   Thumb Code     8  hal_gpio.o(i.hal_gpio_set_output_data)
    hal_gpio_set_pull_state                  0x00016b49   Thumb Code    66  hal_gpio.o(i.hal_gpio_set_pull_state)
    hal_internal_sync_get_hight_performan_mode 0x00016b91   Thumb Code    10  hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode)
    hal_internal_sync_input_resolution_change 0x00016ba1   Thumb Code   336  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    hal_internal_sync_register_lcdc_cb       0x00016d55   Thumb Code     8  hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb)
    hal_internal_vsync_deinit                0x00016d61   Thumb Code    22  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    hal_internal_vsync_get_rx_state          0x00016d81   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state)
    hal_internal_vsync_get_sync_line         0x00016d8d   Thumb Code    16  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    hal_internal_vsync_get_tx_state          0x00016da1   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    hal_internal_vsync_init_rx               0x00016dad   Thumb Code   206  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    hal_internal_vsync_init_tx               0x00016e95   Thumb Code   194  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    hal_internal_vsync_set_rx_state          0x00016f5d   Thumb Code    28  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    hal_internal_vsync_set_tear_mode         0x00016f7d   Thumb Code   298  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    hal_internal_vsync_set_tx_state          0x000170b9   Thumb Code    78  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    hal_intl_dcs_init_sw_fltr                0x00017111   Thumb Code    90  hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr)
    hal_intl_dcs_set_auto_hw_filter          0x000177c5   Thumb Code   130  hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter)
    hal_intl_fb_cal_fb_info                  0x0001787d   Thumb Code   738  hal_internal_fb.o(i.hal_intl_fb_cal_fb_info)
    hal_intl_fb_get_memc_flow_mode           0x00017d21   Thumb Code     6  hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode)
    hal_intl_fb_get_rx_fb_info               0x00017d2d   Thumb Code    12  hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info)
    hal_intl_fb_get_tx_fb_info               0x00017d3d   Thumb Code    12  hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info)
    hal_intl_fb_get_user_flow                0x00017d4d   Thumb Code     6  hal_internal_fb.o(i.hal_intl_fb_get_user_flow)
    hal_intl_svs_deinit_rx                   0x00017d59   Thumb Code    32  hal_internal_svs.o(i.hal_intl_svs_deinit_rx)
    hal_intl_svs_deinit_tx                   0x00017d81   Thumb Code    10  hal_internal_svs.o(i.hal_intl_svs_deinit_tx)
    hal_intl_svs_handle                      0x00017d91   Thumb Code    24  hal_internal_svs.o(i.hal_intl_svs_handle)
    hal_intl_svs_init_rx                     0x00017db5   Thumb Code   120  hal_internal_svs.o(i.hal_intl_svs_init_rx)
    hal_intl_svs_init_tx                     0x00017e35   Thumb Code    16  hal_internal_svs.o(i.hal_intl_svs_init_tx)
    hal_intl_svs_set_rx_vtt                  0x00017e49   Thumb Code     6  hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt)
    hal_intl_svs_update_rxbr_clk             0x00017e55   Thumb Code    52  hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk)
    hal_lcdc_displayproc_config              0x00017e9d   Thumb Code    94  hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config)
    hal_lcdc_postproc_config                 0x00017fbd   Thumb Code   276  hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config)
    hal_lcdc_upscaler_config                 0x00018145   Thumb Code   202  hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config)
    hal_nonshadow_func_update                0x00018225   Thumb Code   180  hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update)
    hal_pwr_enter_deep_sleep_mode            0x000182e1   Thumb Code    42  hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode)
    hal_pwr_enter_normal_sleep_mode          0x0001830b   Thumb Code     8  hal_pwr.o(i.hal_pwr_enter_normal_sleep_mode)
    hal_pwr_enter_stop_sleep_mode            0x00018315   Thumb Code    88  hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode)
    hal_pwr_exit_sleep_mode                  0x00018379   Thumb Code    10  hal_pwr.o(i.hal_pwr_exit_sleep_mode)
    hal_pwr_get_vcc_power_ready              0x00018383   Thumb Code     8  hal_pwr.o(i.hal_pwr_get_vcc_power_ready)
    hal_pwr_set_main_power                   0x0001838b   Thumb Code     8  hal_pwr.o(i.hal_pwr_set_main_power)
    hal_pwr_set_pvd                          0x00018393   Thumb Code     8  hal_pwr.o(i.hal_pwr_set_pvd)
    hal_pwr_set_sleep_mode_power             0x0001839b   Thumb Code     8  hal_pwr.o(i.hal_pwr_set_sleep_mode_power)
    hal_pwr_set_stop_sleep_wakeup_pin        0x000183a5   Thumb Code    86  hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin)
    hal_swire_deinit                         0x00018409   Thumb Code    60  hal_swire.o(i.hal_swire_deinit)
    hal_swire_enable                         0x00018449   Thumb Code    86  hal_swire.o(i.hal_swire_enable)
    hal_swire_init                           0x000184a5   Thumb Code    74  hal_swire.o(i.hal_swire_init)
    hal_swire_set_pulse                      0x000184fd   Thumb Code    32  hal_swire.o(i.hal_swire_set_pulse)
    hal_swire_set_timer                      0x00018521   Thumb Code    60  hal_swire.o(i.hal_swire_set_timer)
    hal_system_enable_systick                0x00018561   Thumb Code     8  hal_system.o(i.hal_system_enable_systick)
    hal_system_get_tick                      0x00018569   Thumb Code     8  hal_system.o(i.hal_system_get_tick)
    hal_system_init                          0x00018571   Thumb Code   192  hal_system.o(i.hal_system_init)
    hal_system_updata_sysclk                 0x00018655   Thumb Code    60  hal_system.o(i.hal_system_updata_sysclk)
    hal_timer_deinit                         0x000186a5   Thumb Code    48  hal_timer.o(i.hal_timer_deinit)
    hal_timer_init                           0x000186d5   Thumb Code    28  hal_timer.o(i.hal_timer_init)
    hal_timer_set_repeat                     0x000186f1   Thumb Code     8  hal_timer.o(i.hal_timer_set_repeat)
    hal_uart_init                            0x00018729   Thumb Code   134  hal_uart.o(i.hal_uart_init)
    hal_uart_send_blocking                   0x000187bd   Thumb Code    24  hal_uart.o(i.hal_uart_send_blocking)
    hal_vsync_func_update                    0x000187d9   Thumb Code    18  hal_dsi_tx_ctrl.o(i.hal_vsync_func_update)
    hal_vsync_reset_lcdc_scaler              0x000187f1   Thumb Code   206  hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler)
    main                                     0x000188d1   Thumb Code    32  main.o(i.main)
    s8_demo                                  0x00018c49   Thumb Code    52  s8_demo.o(i.s8_demo)
    tau_log_init                             0x0001923d   Thumb Code    48  tau_log.o(i.tau_log_init)
    tau_log_printf                           0x00019271   Thumb Code   116  tau_log.o(i.tau_log_printf)
    tau_log_push_log                         0x000192f5   Thumb Code   118  tau_log.o(i.tau_log_push_log)
    panel_init_code                          0x000195a4   Data        7815  s8_demo.o(.constdata)
    Region$$Table$$Base                      0x0001b724   Number         0  anon$$obj.o(Region$$Table)
    Region$$Table$$Limit                     0x0001b744   Number         0  anon$$obj.o(Region$$Table)
    s_swire_pwm_counter                      0x0007000d   Data           1  s8_demo.o(.data)
    t_pps                                    0x0007000e   Data         128  s8_demo.o(.data)
    sg_uart0_tx_handle                       0x00070124   Data           4  hal_uart.o(.data)
    sg_uart0_rx_handle                       0x00070128   Data           4  hal_uart.o(.data)
    sg_uart1_tx_handle                       0x0007012c   Data           4  hal_uart.o(.data)
    sg_uart1_rx_handle                       0x00070130   Data           4  hal_uart.o(.data)
    g_sof_gen_te_func                        0x00070140   Data           4  hal_internal_vsync.o(.data)
    hal_internal_vsync_handle_callback       0x00070144   Data           4  hal_internal_vsync.o(.data)
    hal_internal_disp_end_handle_callback    0x00070148   Data           4  hal_internal_vsync.o(.data)
    g_systick_cb_func                        0x00070174   Data           4  drv_common.o(.data)
    g_system_clock                           0x00070178   Data           4  drv_common.o(.data)
    g_system_delay_step                      0x0007017c   Data           1  drv_common.o(.data)
    dma_req_map                              0x00070280   Data         144  drv_dma.o(.data)
    drv_i2c_table                            0x00070368   Data          36  drv_i2c.o(.data)
    g_int_rxbr_irq0_cb_func                  0x00070394   Data           4  drv_rxbr.o(.data)
    g_int_rxbr_irq1_cb_func                  0x00070398   Data           4  drv_rxbr.o(.data)
    g_int_vidc_cb_func                       0x0007039c   Data           4  drv_vidc.o(.data)
    __stdout                                 0x000703a0   Data           4  stdout.o(.data)
    g_vsync_handle                           0x0007062c   Data          40  hal_internal_vsync.o(.bss)
    sg_pro_motion_handle                     0x00070654   Data          28  hal_internal_vsync.o(.bss)
    g_dcs_execute_table                      0x00070670   Data        2048  hal_internal_dcs.o(.bss)
    g_rx_fb_info                             0x00070f70   Data          68  hal_internal_fb.o(.bss)
    g_packet_fifo                            0x00071048   Data        4204  dcs_packet_fifo.o(.bss)
    __stack_limit                            0x00072118   Data           0  startup_armcm0.o(STACK)
    __initial_sp                             0x00073118   Data           0  startup_armcm0.o(STACK)



==============================================================================

Memory Map of the image

  Image Entry point : 0x000100c1

  Load Region LR_IROM2 (Base: 0x00010000, Size: 0x0000bae8, Max: 0x00010000, ABSOLUTE, COMPRESSED[0x0000b8a4])

    Execution Region ER_IROM2 (Exec base: 0x00010000, Load base: 0x00010000, Size: 0x0000b744, Max: 0x00010000, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00010000   0x00010000   0x000000c0   Data   RO          548    RESET               startup_armcm0.o
    0x000100c0   0x000100c0   0x00000000   Code   RO         2236  * .ARM.Collect$$$$00000000  mc_p.l(entry.o)
    0x000100c0   0x000100c0   0x00000004   Code   RO         2544    .ARM.Collect$$$$00000001  mc_p.l(entry2.o)
    0x000100c4   0x000100c4   0x00000004   Code   RO         2547    .ARM.Collect$$$$00000004  mc_p.l(entry5.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         2549    .ARM.Collect$$$$00000008  mc_p.l(entry7b.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         2551    .ARM.Collect$$$$0000000A  mc_p.l(entry8b.o)
    0x000100c8   0x000100c8   0x00000008   Code   RO         2552    .ARM.Collect$$$$0000000B  mc_p.l(entry9a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         2554    .ARM.Collect$$$$0000000D  mc_p.l(entry10a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         2556    .ARM.Collect$$$$0000000F  mc_p.l(entry11a.o)
    0x000100d0   0x000100d0   0x00000004   Code   RO         2545    .ARM.Collect$$$$00002712  mc_p.l(entry2.o)
    0x000100d4   0x000100d4   0x00000078   Code   RO          549    .text               startup_armcm0.o
    0x0001014c   0x0001014c   0x0000002c   Code   RO         2239    .text               mc_p.l(uidiv.o)
    0x00010178   0x00010178   0x00000028   Code   RO         2241    .text               mc_p.l(idiv.o)
    0x000101a0   0x000101a0   0x00000024   Code   RO         2243    .text               mc_p.l(memcpya.o)
    0x000101c4   0x000101c4   0x00000024   Code   RO         2245    .text               mc_p.l(memseta.o)
    0x000101e8   0x000101e8   0x0000000e   Code   RO         2247    .text               mc_p.l(strlen.o)
    0x000101f6   0x000101f6   0x0000001a   Code   RO         2249    .text               mc_p.l(memcmp.o)
    0x00010210   0x00010210   0x000000b2   Code   RO         2514    .text               mf_p.l(fadd.o)
    0x000102c2   0x000102c2   0x0000007a   Code   RO         2516    .text               mf_p.l(fmul.o)
    0x0001033c   0x0001033c   0x0000007c   Code   RO         2518    .text               mf_p.l(fdiv.o)
    0x000103b8   0x000103b8   0x00000018   Code   RO         2520    .text               mf_p.l(fscalb.o)
    0x000103d0   0x000103d0   0x00000164   Code   RO         2522    .text               mf_p.l(dadd.o)
    0x00010534   0x00010534   0x000000d0   Code   RO         2524    .text               mf_p.l(dmul.o)
    0x00010604   0x00010604   0x000000f0   Code   RO         2526    .text               mf_p.l(ddiv.o)
    0x000106f4   0x000106f4   0x0000000e   Code   RO         2528    .text               mf_p.l(ffltui.o)
    0x00010702   0x00010702   0x00000002   PAD
    0x00010704   0x00010704   0x0000001c   Code   RO         2530    .text               mf_p.l(dfltui.o)
    0x00010720   0x00010720   0x00000028   Code   RO         2532    .text               mf_p.l(ffixui.o)
    0x00010748   0x00010748   0x0000003c   Code   RO         2534    .text               mf_p.l(dfixui.o)
    0x00010784   0x00010784   0x00000028   Code   RO         2536    .text               mf_p.l(f2d.o)
    0x000107ac   0x000107ac   0x00000038   Code   RO         2538    .text               mf_p.l(d2f.o)
    0x000107e4   0x000107e4   0x00000014   Code   RO         2540    .text               mf_p.l(cfcmple.o)
    0x000107f8   0x000107f8   0x00000014   Code   RO         2542    .text               mf_p.l(cfrcmple.o)
    0x0001080c   0x0001080c   0x00000060   Code   RO         2559    .text               mc_p.l(uldiv.o)
    0x0001086c   0x0001086c   0x00000020   Code   RO         2561    .text               mc_p.l(llshl.o)
    0x0001088c   0x0001088c   0x00000022   Code   RO         2563    .text               mc_p.l(llushr.o)
    0x000108ae   0x000108ae   0x00000026   Code   RO         2565    .text               mc_p.l(llsshr.o)
    0x000108d4   0x000108d4   0x00000000   Code   RO         2567    .text               mc_p.l(iusefp.o)
    0x000108d4   0x000108d4   0x00000082   Code   RO         2568    .text               mf_p.l(fepilogue.o)
    0x00010956   0x00010956   0x000000be   Code   RO         2570    .text               mf_p.l(depilogue.o)
    0x00010a14   0x00010a14   0x00000040   Code   RO         2574    .text               mf_p.l(dfixul.o)
    0x00010a54   0x00010a54   0x00000028   Code   RO         2576    .text               mf_p.l(cdrcmple.o)
    0x00010a7c   0x00010a7c   0x00000024   Code   RO         2578    .text               mc_p.l(init.o)
    0x00010aa0   0x00010aa0   0x00000056   Code   RO         2588    .text               mc_p.l(__dczerorl2.o)
    0x00010af6   0x00010af6   0x00000002   PAD
    0x00010af8   0x00010af8   0x0000001c   Code   RO         1294    i.AP_NRESET_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010b14   0x00010b14   0x0000005c   Code   RO         1219    i.DMA_IRQn_Handler  CVWL668.lib(drv_dma.o)
    0x00010b70   0x00010b70   0x0000000a   Code   RO         1295    i.EXTI_INT0_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010b7a   0x00010b7a   0x0000000a   Code   RO         1296    i.EXTI_INT1_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010b84   0x00010b84   0x0000000a   Code   RO         1297    i.EXTI_INT2_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010b8e   0x00010b8e   0x0000000a   Code   RO         1298    i.EXTI_INT3_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010b98   0x00010b98   0x0000000a   Code   RO         1299    i.EXTI_INT4_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010ba2   0x00010ba2   0x0000000a   Code   RO         1300    i.EXTI_INT5_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010bac   0x00010bac   0x0000000a   Code   RO         1301    i.EXTI_INT6_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010bb6   0x00010bb6   0x0000000a   Code   RO         1302    i.EXTI_INT7_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010bc0   0x00010bc0   0x00000048   Code   RO         1154    i.HardFault_Handler  CVWL668.lib(drv_common.o)
    0x00010c08   0x00010c08   0x0000000c   Code   RO         1550    i.I2C0_IRQn_Handler  CVWL668.lib(drv_i2c.o)
    0x00010c14   0x00010c14   0x0000000c   Code   RO         1551    i.I2C1_IRQn_Handler  CVWL668.lib(drv_i2c.o)
    0x00010c20   0x00010c20   0x0000000c   Code   RO         1552    i.I2C2_IRQn_Handler  CVWL668.lib(drv_i2c.o)
    0x00010c2c   0x00010c2c   0x00000100   Code   RO          999    i.LCDC_IRQn_Handler  CVWL668.lib(hal_internal_vsync.o)
    0x00010d2c   0x00010d2c   0x0000009a   Code   RO         1918    i.MEMC_IRQn_Handler  CVWL668.lib(drv_memc.o)
    0x00010dc6   0x00010dc6   0x00000002   PAD
    0x00010dc8   0x00010dc8   0x000000b8   Code   RO         1724    i.MIPI_TX_IRQn_Handler  CVWL668.lib(drv_dsi_tx.o)
    0x00010e80   0x00010e80   0x000000b4   Code   RO          321    i.PhoneDisOffDeal   s8_demo.o
    0x00010f34   0x00010f34   0x00000048   Code   RO          817    i.SPIM_IRQn_Handler  CVWL668.lib(hal_spi_master.o)
    0x00010f7c   0x00010f7c   0x00000030   Code   RO         1474    i.SWIRE_IRQn_Handler  CVWL668.lib(drv_swire.o)
    0x00010fac   0x00010fac   0x00000018   Code   RO         1155    i.SysTick_Handler   CVWL668.lib(drv_common.o)
    0x00010fc4   0x00010fc4   0x0000000a   Code   RO         1517    i.TIMER0_IRQn_Handler  CVWL668.lib(drv_timer.o)
    0x00010fce   0x00010fce   0x0000000a   Code   RO         1518    i.TIMER1_IRQn_Handler  CVWL668.lib(drv_timer.o)
    0x00010fd8   0x00010fd8   0x0000000a   Code   RO         1519    i.TIMER2_IRQn_Handler  CVWL668.lib(drv_timer.o)
    0x00010fe2   0x00010fe2   0x0000000a   Code   RO         1520    i.TIMER3_IRQn_Handler  CVWL668.lib(drv_timer.o)
    0x00010fec   0x00010fec   0x0000000e   Code   RO         2582    i.__scatterload_copy  mc_p.l(handlers.o)
    0x00010ffa   0x00010ffa   0x00000002   Code   RO         2583    i.__scatterload_null  mc_p.l(handlers.o)
    0x00010ffc   0x00010ffc   0x00000004   PAD
    0x00011000   0x00011000   0x0000001c   Data   RO         1162    .ARM.__at_0x11000   CVWL668.lib(drv_common.o)
    0x0001101c   0x0001101c   0x00000010   Data   RO          955    .ARM.__at_0x1101C   CVWL668.lib(tau_log.o)
    0x0001102c   0x0001102c   0x00000016   Data   RO          686    .ARM.__at_0x1102C   CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00011042   0x00011042   0x00000002   PAD
    0x00011044   0x00011044   0x00000364   Code   RO         1663    i.MIPI_RX_IRQn_Handler  CVWL668.lib(drv_dsi_rx.o)
    0x000113a8   0x000113a8   0x00000180   Code   RO         2158    i.UART_IRQn_Handler  CVWL668.lib(drv_uart.o)
    0x00011528   0x00011528   0x0000001c   Code   RO         2073    i.VIDC_IRQn_Handler  CVWL668.lib(drv_vidc.o)
    0x00011544   0x00011544   0x0000001c   Code   RO         1984    i.VPRE1_IRQn_Handler  CVWL668.lib(drv_rxbr.o)
    0x00011560   0x00011560   0x0000006c   Code   RO         1065    i.VPRE_IRQn_Handler  CVWL668.lib(hal_internal_dcs.o)
    0x000115cc   0x000115cc   0x00000020   Code   RO         2486    i.__0printf         mc_p.l(printfa.o)
    0x000115ec   0x000115ec   0x00000024   Code   RO         2492    i.__0vsprintf       mc_p.l(printfa.o)
    0x00011610   0x00011610   0x0000002e   Code   RO         2572    i.__ARM_clz         mf_p.l(depilogue.o)
    0x0001163e   0x0001163e   0x0000001a   Code   RO          633    i.__ARM_common_switch8  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00011658   0x00011658   0x00000020   Code   RO         1985    i.__NVIC_DisableIRQ  CVWL668.lib(drv_rxbr.o)
    0x00011678   0x00011678   0x00000018   Code   RO         1986    i.__NVIC_EnableIRQ  CVWL668.lib(drv_rxbr.o)
    0x00011690   0x00011690   0x0000000e   Code   RO         2584    i.__scatterload_zeroinit  mc_p.l(handlers.o)
    0x0001169e   0x0001169e   0x00000002   PAD
    0x000116a0   0x000116a0   0x00000174   Code   RO         2493    i._fp_digits        mc_p.l(printfa.o)
    0x00011814   0x00011814   0x000006ec   Code   RO         2494    i._printf_core      mc_p.l(printfa.o)
    0x00011f00   0x00011f00   0x00000020   Code   RO         2495    i._printf_post_padding  mc_p.l(printfa.o)
    0x00011f20   0x00011f20   0x0000002c   Code   RO         2496    i._printf_pre_padding  mc_p.l(printfa.o)
    0x00011f4c   0x00011f4c   0x0000000a   Code   RO         2498    i._sputc            mc_p.l(printfa.o)
    0x00011f56   0x00011f56   0x00000002   PAD
    0x00011f58   0x00011f58   0x00000020   Code   RO          323    i.ap_dcs_set_AOD_53  s8_demo.o
    0x00011f78   0x00011f78   0x000000c0   Code   RO          324    i.ap_dcs_set_backlight  s8_demo.o
    0x00012038   0x00012038   0x00000006   Code   RO          325    i.ap_dcs_set_display_off  s8_demo.o
    0x0001203e   0x0001203e   0x00000002   PAD
    0x00012040   0x00012040   0x0000003c   Code   RO          326    i.ap_dcs_set_display_on  s8_demo.o
    0x0001207c   0x0001207c   0x00000054   Code   RO          327    i.ap_dcs_set_enter_sleep_mode  s8_demo.o
    0x000120d0   0x000120d0   0x0000004c   Code   RO          328    i.ap_dcs_set_exit_sleep_mode  s8_demo.o
    0x0001211c   0x0001211c   0x0000005c   Code   RO          330    i.ap_rstn_pull_down_cb  s8_demo.o
    0x00012178   0x00012178   0x00000054   Code   RO          331    i.ap_rstn_pull_high_cb  s8_demo.o
    0x000121cc   0x000121cc   0x00000018   Code   RO          332    i.ap_set_framerate  s8_demo.o
    0x000121e4   0x000121e4   0x00000084   Code   RO          333    i.ap_update_pps_9E  s8_demo.o
    0x00012268   0x00012268   0x0000002c   Code   RO          334    i.app_display_init  s8_demo.o
    0x00012294   0x00012294   0x00000020   Code   RO          335    i.app_gpio_init     s8_demo.o
    0x000122b4   0x000122b4   0x00000044   Code   RO          336    i.app_init_panel    s8_demo.o
    0x000122f8   0x000122f8   0x000000e8   Code   RO          337    i.app_mipi_rx_init  s8_demo.o
    0x000123e0   0x000123e0   0x000000c0   Code   RO          339    i.app_mipi_tx_init  s8_demo.o
    0x000124a0   0x000124a0   0x0000006c   Code   RO          340    i.app_mipi_tx_start  s8_demo.o
    0x0001250c   0x0001250c   0x0000008c   Code   RO          341    i.app_set_dcs_hw_ack  s8_demo.o
    0x00012598   0x00012598   0x00000034   Code   RO          342    i.app_system_process  s8_demo.o
    0x000125cc   0x000125cc   0x00000048   Code   RO          343    i.app_system_resume  s8_demo.o
    0x00012614   0x00012614   0x0000012c   Code   RO          344    i.app_system_suspend  s8_demo.o
    0x00012740   0x00012740   0x0000002e   Code   RO          345    i.app_tx_panel_reset  s8_demo.o
    0x0001276e   0x0001276e   0x00000002   PAD
    0x00012770   0x00012770   0x00000020   Code   RO          528    i.board_Init        board.o
    0x00012790   0x00012790   0x000000c8   Code   RO         2233    i.ceil              m_ps.l(ceil.o)
    0x00012858   0x00012858   0x0000002c   Code   RO         1000    i.check_mipi_rx_tx_video_info  CVWL668.lib(hal_internal_vsync.o)
    0x00012884   0x00012884   0x00000088   Code   RO         1066    i.check_pkt_buf_rev  CVWL668.lib(hal_internal_dcs.o)
    0x0001290c   0x0001290c   0x00000058   Code   RO         1629    i.dcs_packet_fifo_alloc  CVWL668.lib(dcs_packet_fifo.o)
    0x00012964   0x00012964   0x00000018   Code   RO         1630    i.dcs_packet_fifo_init  CVWL668.lib(dcs_packet_fifo.o)
    0x0001297c   0x0001297c   0x00000044   Code   RO         1631    i.dcs_packet_free_fifo_header  CVWL668.lib(dcs_packet_fifo.o)
    0x000129c0   0x000129c0   0x00000024   Code   RO         1632    i.dcs_packet_get_fifo_header  CVWL668.lib(dcs_packet_fifo.o)
    0x000129e4   0x000129e4   0x00000018   Code   RO          942    i.delayMs           CVWL668.lib(tau_delay.o)
    0x000129fc   0x000129fc   0x0000002c   Code   RO          943    i.delayUs           CVWL668.lib(tau_delay.o)
    0x00012a28   0x00012a28   0x00000058   Code   RO         1157    i.drv_common_enable_systick  CVWL668.lib(drv_common.o)
    0x00012a80   0x00012a80   0x0000000c   Code   RO         1158    i.drv_common_get_tick  CVWL668.lib(drv_common.o)
    0x00012a8c   0x00012a8c   0x00000008   Code   RO         1160    i.drv_common_system_init  CVWL668.lib(drv_common.o)
    0x00012a94   0x00012a94   0x0000003c   Code   RO         1179    i.drv_crgu_enable_clock  CVWL668.lib(drv_crgu.o)
    0x00012ad0   0x00012ad0   0x00000068   Code   RO         1182    i.drv_crgu_get_rxbr_clk  CVWL668.lib(drv_crgu.o)
    0x00012b38   0x00012b38   0x00000010   Code   RO         1185    i.drv_crgu_reset_modules  CVWL668.lib(drv_crgu.o)
    0x00012b48   0x00012b48   0x00000028   Code   RO         1186    i.drv_crgu_set_ahb_clk  CVWL668.lib(drv_crgu.o)
    0x00012b70   0x00012b70   0x00000010   Code   RO         1187    i.drv_crgu_set_clock_div  CVWL668.lib(drv_crgu.o)
    0x00012b80   0x00012b80   0x0000003c   Code   RO         1189    i.drv_crgu_set_dpi_clk  CVWL668.lib(drv_crgu.o)
    0x00012bbc   0x00012bbc   0x00000038   Code   RO         1190    i.drv_crgu_set_dsc_clk  CVWL668.lib(drv_crgu.o)
    0x00012bf4   0x00012bf4   0x00000028   Code   RO         1191    i.drv_crgu_set_fb_clk  CVWL668.lib(drv_crgu.o)
    0x00012c1c   0x00012c1c   0x00000028   Code   RO         1192    i.drv_crgu_set_lcdc_clk  CVWL668.lib(drv_crgu.o)
    0x00012c44   0x00012c44   0x00000018   Code   RO         1193    i.drv_crgu_set_reset  CVWL668.lib(drv_crgu.o)
    0x00012c5c   0x00012c5c   0x00000028   Code   RO         1194    i.drv_crgu_set_rxbr_clk  CVWL668.lib(drv_crgu.o)
    0x00012c84   0x00012c84   0x00000028   Code   RO         1195    i.drv_crgu_set_vidc_clk  CVWL668.lib(drv_crgu.o)
    0x00012cac   0x00012cac   0x00000018   Code   RO         1221    i.drv_dma_clear_status  CVWL668.lib(drv_dma.o)
    0x00012cc4   0x00012cc4   0x00000014   Code   RO         1227    i.drv_dma_get_int_source  CVWL668.lib(drv_dma.o)
    0x00012cd8   0x00012cd8   0x0000001c   Code   RO         1282    i.drv_dsc_dec_disable  CVWL668.lib(drv_dsc_dec.o)
    0x00012cf4   0x00012cf4   0x00000038   Code   RO         1283    i.drv_dsc_dec_enable  CVWL668.lib(drv_dsc_dec.o)
    0x00012d2c   0x00012d2c   0x00000020   Code   RO         1284    i.drv_dsc_dec_get_nslc  CVWL668.lib(drv_dsc_dec.o)
    0x00012d4c   0x00012d4c   0x0000001c   Code   RO         1285    i.drv_dsc_dec_set_irqen  CVWL668.lib(drv_dsc_dec.o)
    0x00012d68   0x00012d68   0x0000010c   Code   RO         1664    i.drv_dsi_rx_calc_ipi_tx_delay  CVWL668.lib(drv_dsi_rx.o)
    0x00012e74   0x00012e74   0x00000040   Code   RO         1665    i.drv_dsi_rx_enable_irq  CVWL668.lib(drv_dsi_rx.o)
    0x00012eb4   0x00012eb4   0x00000050   Code   RO         1667    i.drv_dsi_rx_get_color_bpp  CVWL668.lib(drv_dsi_rx.o)
    0x00012f04   0x00012f04   0x0000001c   Code   RO         1668    i.drv_dsi_rx_get_color_pcc  CVWL668.lib(drv_dsi_rx.o)
    0x00012f20   0x00012f20   0x00000010   Code   RO         1669    i.drv_dsi_rx_get_compression_en  CVWL668.lib(drv_dsi_rx.o)
    0x00012f30   0x00012f30   0x00000010   Code   RO         1670    i.drv_dsi_rx_get_ddi_crc_en  CVWL668.lib(drv_dsi_rx.o)
    0x00012f40   0x00012f40   0x00000018   Code   RO         1675    i.drv_dsi_rx_power_up  CVWL668.lib(drv_dsi_rx.o)
    0x00012f58   0x00012f58   0x0000001c   Code   RO         1676    i.drv_dsi_rx_set_check_crc  CVWL668.lib(drv_dsi_rx.o)
    0x00012f74   0x00012f74   0x00000024   Code   RO         1677    i.drv_dsi_rx_set_ctrl_cfg  CVWL668.lib(drv_dsi_rx.o)
    0x00012f98   0x00012f98   0x00000010   Code   RO         1678    i.drv_dsi_rx_set_ddi_cfg  CVWL668.lib(drv_dsi_rx.o)
    0x00012fa8   0x00012fa8   0x0000001c   Code   RO         1679    i.drv_dsi_rx_set_ddi_crc_en  CVWL668.lib(drv_dsi_rx.o)
    0x00012fc4   0x00012fc4   0x0000000c   Code   RO         1682    i.drv_dsi_rx_set_inten  CVWL668.lib(drv_dsi_rx.o)
    0x00012fd0   0x00012fd0   0x00000010   Code   RO         1683    i.drv_dsi_rx_set_ipi_cfg  CVWL668.lib(drv_dsi_rx.o)
    0x00012fe0   0x00012fe0   0x0000001c   Code   RO         1685    i.drv_dsi_rx_set_ipi_ycbcr_frmt  CVWL668.lib(drv_dsi_rx.o)
    0x00012ffc   0x00012ffc   0x00000014   Code   RO         1686    i.drv_dsi_rx_set_lane_swap  CVWL668.lib(drv_dsi_rx.o)
    0x00013010   0x00013010   0x00000024   Code   RO         1687    i.drv_dsi_rx_set_resp_cnt  CVWL668.lib(drv_dsi_rx.o)
    0x00013034   0x00013034   0x0000001c   Code   RO         1688    i.drv_dsi_rx_set_tear_resp_en  CVWL668.lib(drv_dsi_rx.o)
    0x00013050   0x00013050   0x00000100   Code   RO         1689    i.drv_dsi_rx_set_up_phy  CVWL668.lib(drv_dsi_rx.o)
    0x00013150   0x00013150   0x00000018   Code   RO         1690    i.drv_dsi_rx_shut_down  CVWL668.lib(drv_dsi_rx.o)
    0x00013168   0x00013168   0x00000018   Code   RO         1726    i.drv_dsi_tx_command_header  CVWL668.lib(drv_dsi_tx.o)
    0x00013180   0x00013180   0x00000058   Code   RO         1727    i.drv_dsi_tx_command_mode_cfg  CVWL668.lib(drv_dsi_tx.o)
    0x000131d8   0x000131d8   0x0000000c   Code   RO         1728    i.drv_dsi_tx_command_put_payload  CVWL668.lib(drv_dsi_tx.o)
    0x000131e4   0x000131e4   0x00000020   Code   RO         1729    i.drv_dsi_tx_config_eotp  CVWL668.lib(drv_dsi_tx.o)
    0x00013204   0x00013204   0x0000000c   Code   RO         1730    i.drv_dsi_tx_config_int  CVWL668.lib(drv_dsi_tx.o)
    0x00013210   0x00013210   0x00000010   Code   RO         1731    i.drv_dsi_tx_dpi_lpcmd_time  CVWL668.lib(drv_dsi_tx.o)
    0x00013220   0x00013220   0x00000010   Code   RO         1732    i.drv_dsi_tx_dpi_mode  CVWL668.lib(drv_dsi_tx.o)
    0x00013230   0x00013230   0x00000024   Code   RO         1733    i.drv_dsi_tx_dpi_polarity  CVWL668.lib(drv_dsi_tx.o)
    0x00013254   0x00013254   0x0000000c   Code   RO         1734    i.drv_dsi_tx_edpi_cmd_size  CVWL668.lib(drv_dsi_tx.o)
    0x00013260   0x00013260   0x0000000c   Code   RO         1736    i.drv_dsi_tx_get_cmd_status  CVWL668.lib(drv_dsi_tx.o)
    0x0001326c   0x0001326c   0x0000000c   Code   RO         1738    i.drv_dsi_tx_mode   CVWL668.lib(drv_dsi_tx.o)
    0x00013278   0x00013278   0x0000001c   Code   RO         1739    i.drv_dsi_tx_phy_clock_lane_auto_lp  CVWL668.lib(drv_dsi_tx.o)
    0x00013294   0x00013294   0x00000020   Code   RO         1740    i.drv_dsi_tx_phy_clock_lane_req_hs  CVWL668.lib(drv_dsi_tx.o)
    0x000132b4   0x000132b4   0x00000010   Code   RO         1742    i.drv_dsi_tx_phy_lane_mode  CVWL668.lib(drv_dsi_tx.o)
    0x000132c4   0x000132c4   0x00000068   Code   RO         1745    i.drv_dsi_tx_phy_status_ready  CVWL668.lib(drv_dsi_tx.o)
    0x0001332c   0x0001332c   0x00000044   Code   RO         1746    i.drv_dsi_tx_phy_status_stopstate  CVWL668.lib(drv_dsi_tx.o)
    0x00013370   0x00013370   0x00000150   Code   RO         1748    i.drv_dsi_tx_phy_test_setup  CVWL668.lib(drv_dsi_tx.o)
    0x000134c0   0x000134c0   0x00000020   Code   RO         1749    i.drv_dsi_tx_phy_time_cfg  CVWL668.lib(drv_dsi_tx.o)
    0x000134e0   0x000134e0   0x0000000c   Code   RO         1753    i.drv_dsi_tx_powerup  CVWL668.lib(drv_dsi_tx.o)
    0x000134ec   0x000134ec   0x00000024   Code   RO         1754    i.drv_dsi_tx_response_mode  CVWL668.lib(drv_dsi_tx.o)
    0x00013510   0x00013510   0x0000001c   Code   RO         1757    i.drv_dsi_tx_set_bta_ack  CVWL668.lib(drv_dsi_tx.o)
    0x0001352c   0x0001352c   0x00000014   Code   RO         1758    i.drv_dsi_tx_set_esc_div  CVWL668.lib(drv_dsi_tx.o)
    0x00013540   0x00013540   0x00000040   Code   RO         1759    i.drv_dsi_tx_set_int  CVWL668.lib(drv_dsi_tx.o)
    0x00013580   0x00013580   0x00000018   Code   RO         1760    i.drv_dsi_tx_set_time_out_div  CVWL668.lib(drv_dsi_tx.o)
    0x00013598   0x00013598   0x00000014   Code   RO         1761    i.drv_dsi_tx_set_video_chunk  CVWL668.lib(drv_dsi_tx.o)
    0x000135ac   0x000135ac   0x00000024   Code   RO         1762    i.drv_dsi_tx_set_video_timing  CVWL668.lib(drv_dsi_tx.o)
    0x000135d0   0x000135d0   0x0000000c   Code   RO         1764    i.drv_dsi_tx_shutdown  CVWL668.lib(drv_dsi_tx.o)
    0x000135dc   0x000135dc   0x0000002c   Code   RO         1765    i.drv_dsi_tx_timeout_cfg  CVWL668.lib(drv_dsi_tx.o)
    0x00013608   0x00013608   0x000000e8   Code   RO         1768    i.drv_dsi_tx_video_mode_cfg  CVWL668.lib(drv_dsi_tx.o)
    0x000136f0   0x000136f0   0x00000036   Code   RO         2203    i.drv_efuse_enter_inactive  CVWL668.lib(drv_efuse.o)
    0x00013726   0x00013726   0x0000000c   Code   RO         2206    i.drv_efuse_int_enable  CVWL668.lib(drv_efuse.o)
    0x00013732   0x00013732   0x0000003a   Code   RO         2207    i.drv_efuse_read    CVWL668.lib(drv_efuse.o)
    0x0001376c   0x0001376c   0x00000018   Code   RO         2208    i.drv_efuse_read_req  CVWL668.lib(drv_efuse.o)
    0x00013784   0x00013784   0x00000010   Code   RO         1303    i.drv_gpio_get_attribute  CVWL668.lib(drv_gpio.o)
    0x00013794   0x00013794   0x00000018   Code   RO         1304    i.drv_gpio_get_input_data  CVWL668.lib(drv_gpio.o)
    0x000137ac   0x000137ac   0x00000024   Code   RO         1305    i.drv_gpio_handle_int  CVWL668.lib(drv_gpio.o)
    0x000137d0   0x000137d0   0x0000000c   Code   RO         1306    i.drv_gpio_register_ap_reset_callback  CVWL668.lib(drv_gpio.o)
    0x000137dc   0x000137dc   0x00000014   Code   RO         1307    i.drv_gpio_register_callback  CVWL668.lib(drv_gpio.o)
    0x000137f0   0x000137f0   0x0000001c   Code   RO         1308    i.drv_gpio_set_attribute  CVWL668.lib(drv_gpio.o)
    0x0001380c   0x0001380c   0x00000044   Code   RO         1309    i.drv_gpio_set_int  CVWL668.lib(drv_gpio.o)
    0x00013850   0x00013850   0x00000020   Code   RO         1310    i.drv_gpio_set_ioe  CVWL668.lib(drv_gpio.o)
    0x00013870   0x00013870   0x00000014   Code   RO         1311    i.drv_gpio_set_mode  CVWL668.lib(drv_gpio.o)
    0x00013884   0x00013884   0x00000020   Code   RO          743    i.drv_gpio_set_output_data  CVWL668.lib(hal_gpio.o)
    0x000138a4   0x000138a4   0x00000028   Code   RO         1830    i.drv_lcdc_bcsa_config  CVWL668.lib(drv_lcdc.o)
    0x000138cc   0x000138cc   0x0000002c   Code   RO         1831    i.drv_lcdc_cfg_int_frame  CVWL668.lib(drv_lcdc.o)
    0x000138f8   0x000138f8   0x00000018   Code   RO         1832    i.drv_lcdc_clear_int  CVWL668.lib(drv_lcdc.o)
    0x00013910   0x00013910   0x00000034   Code   RO         1834    i.drv_lcdc_cmd_start  CVWL668.lib(drv_lcdc.o)
    0x00013944   0x00013944   0x00000014   Code   RO         1835    i.drv_lcdc_config_acc_command_mode  CVWL668.lib(drv_lcdc.o)
    0x00013958   0x00013958   0x00000038   Code   RO         1836    i.drv_lcdc_config_int  CVWL668.lib(drv_lcdc.o)
    0x00013990   0x00013990   0x00000028   Code   RO         1837    i.drv_lcdc_config_int_single  CVWL668.lib(drv_lcdc.o)
    0x000139b8   0x000139b8   0x00000018   Code   RO         1838    i.drv_lcdc_config_overwrite_rgb  CVWL668.lib(drv_lcdc.o)
    0x000139d0   0x000139d0   0x00000050   Code   RO         1839    i.drv_lcdc_config_src_parameter  CVWL668.lib(drv_lcdc.o)
    0x00013a20   0x00013a20   0x00000010   Code   RO         1840    i.drv_lcdc_crop_hact  CVWL668.lib(drv_lcdc.o)
    0x00013a30   0x00013a30   0x00000038   Code   RO         1841    i.drv_lcdc_ctrl_flow  CVWL668.lib(drv_lcdc.o)
    0x00013a68   0x00013a68   0x00000030   Code   RO         1842    i.drv_lcdc_dith_config  CVWL668.lib(drv_lcdc.o)
    0x00013a98   0x00013a98   0x0000003c   Code   RO         1844    i.drv_lcdc_edge_dect_config  CVWL668.lib(drv_lcdc.o)
    0x00013ad4   0x00013ad4   0x00000064   Code   RO         1845    i.drv_lcdc_edge_enh_config  CVWL668.lib(drv_lcdc.o)
    0x00013b38   0x00013b38   0x00000024   Code   RO         1846    i.drv_lcdc_enable_shadow_reg  CVWL668.lib(drv_lcdc.o)
    0x00013b5c   0x00013b5c   0x0000001c   Code   RO         1847    i.drv_lcdc_endianness_config  CVWL668.lib(drv_lcdc.o)
    0x00013b78   0x00013b78   0x00000020   Code   RO         1848    i.drv_lcdc_fc_config  CVWL668.lib(drv_lcdc.o)
    0x00013b98   0x00013b98   0x00000024   Code   RO         1850    i.drv_lcdc_fldc_config  CVWL668.lib(drv_lcdc.o)
    0x00013bbc   0x00013bbc   0x00000024   Code   RO         1851    i.drv_lcdc_function_disable  CVWL668.lib(drv_lcdc.o)
    0x00013be0   0x00013be0   0x00000024   Code   RO         1852    i.drv_lcdc_function_enable  CVWL668.lib(drv_lcdc.o)
    0x00013c04   0x00013c04   0x0000003c   Code   RO         1863    i.drv_lcdc_set_int  CVWL668.lib(drv_lcdc.o)
    0x00013c40   0x00013c40   0x0000001c   Code   RO         1864    i.drv_lcdc_set_prefetch  CVWL668.lib(drv_lcdc.o)
    0x00013c5c   0x00013c5c   0x0000001c   Code   RO         1865    i.drv_lcdc_set_tear_line  CVWL668.lib(drv_lcdc.o)
    0x00013c78   0x00013c78   0x00000010   Code   RO         1867    i.drv_lcdc_stop_display  CVWL668.lib(drv_lcdc.o)
    0x00013c88   0x00013c88   0x0000003c   Code   RO         1869    i.drv_lcdc_vid_hw_start  CVWL668.lib(drv_lcdc.o)
    0x00013cc4   0x00013cc4   0x00000018   Code   RO         1871    i.drv_lcdc_vintp_mode_config  CVWL668.lib(drv_lcdc.o)
    0x00013cdc   0x00013cdc   0x00000014   Code   RO         1919    i.drv_memc_clear_status  CVWL668.lib(drv_memc.o)
    0x00013cf0   0x00013cf0   0x00000040   Code   RO         1920    i.drv_memc_enable_irq  CVWL668.lib(drv_memc.o)
    0x00013d30   0x00013d30   0x00000010   Code   RO         1921    i.drv_memc_gen_a_tear_signal  CVWL668.lib(drv_memc.o)
    0x00013d40   0x00013d40   0x00000018   Code   RO         1922    i.drv_memc_get_status  CVWL668.lib(drv_memc.o)
    0x00013d58   0x00013d58   0x00000010   Code   RO         1923    i.drv_memc_get_tear_mode  CVWL668.lib(drv_memc.o)
    0x00013d68   0x00013d68   0x0000001c   Code   RO         1924    i.drv_memc_rate_transfer_sel  CVWL668.lib(drv_memc.o)
    0x00013d84   0x00013d84   0x00000014   Code   RO         1925    i.drv_memc_sel_vsync  CVWL668.lib(drv_memc.o)
    0x00013d98   0x00013d98   0x00000018   Code   RO         1926    i.drv_memc_set_active_height  CVWL668.lib(drv_memc.o)
    0x00013db0   0x00013db0   0x0000001c   Code   RO         1927    i.drv_memc_set_circ_mode_enable  CVWL668.lib(drv_memc.o)
    0x00013dcc   0x00013dcc   0x00000014   Code   RO         1928    i.drv_memc_set_data_mode  CVWL668.lib(drv_memc.o)
    0x00013de0   0x00013de0   0x00000018   Code   RO         1931    i.drv_memc_set_double_buffer  CVWL668.lib(drv_memc.o)
    0x00013df8   0x00013df8   0x0000001c   Code   RO         1935    i.drv_memc_set_frame_drop_select  CVWL668.lib(drv_memc.o)
    0x00013e14   0x00013e14   0x00000018   Code   RO         1936    i.drv_memc_set_fs_en_conditions  CVWL668.lib(drv_memc.o)
    0x00013e2c   0x00013e2c   0x0000001c   Code   RO         1938    i.drv_memc_set_lcdc_st_conditions  CVWL668.lib(drv_memc.o)
    0x00013e48   0x00013e48   0x00000020   Code   RO         1939    i.drv_memc_set_ltpo_mode  CVWL668.lib(drv_memc.o)
    0x00013e68   0x00013e68   0x00000018   Code   RO         1940    i.drv_memc_set_ltpo_pu_thres  CVWL668.lib(drv_memc.o)
    0x00013e80   0x00013e80   0x00000014   Code   RO         1944    i.drv_memc_set_tear_mode  CVWL668.lib(drv_memc.o)
    0x00013e94   0x00013e94   0x0000002c   Code   RO         1945    i.drv_memc_set_tear_waveform  CVWL668.lib(drv_memc.o)
    0x00013ec0   0x00013ec0   0x00000014   Code   RO         1947    i.drv_memc_set_vidc_sync_cnt  CVWL668.lib(drv_memc.o)
    0x00013ed4   0x00013ed4   0x00000010   Code   RO         2226    i.drv_phy_test_clear  CVWL668.lib(drv_phy_common.o)
    0x00013ee4   0x00013ee4   0x00000018   Code   RO         2227    i.drv_phy_test_lock  CVWL668.lib(drv_phy_common.o)
    0x00013efc   0x00013efc   0x00000030   Code   RO         1341    i.drv_pwr_efuse_pd  CVWL668.lib(drv_pwr.o)
    0x00013f2c   0x00013f2c   0x0000004c   Code   RO         1343    i.drv_pwr_enter_deep_sleep_mode  CVWL668.lib(drv_pwr.o)
    0x00013f78   0x00013f78   0x00000034   Code   RO         1345    i.drv_pwr_enter_sleep_mode_ex  CVWL668.lib(drv_pwr.o)
    0x00013fac   0x00013fac   0x00000098   Code   RO         1346    i.drv_pwr_enter_stop_sleep_mode  CVWL668.lib(drv_pwr.o)
    0x00014044   0x00014044   0x00000028   Code   RO         1347    i.drv_pwr_exit_sleep_mode  CVWL668.lib(drv_pwr.o)
    0x0001406c   0x0001406c   0x00000010   Code   RO         1350    i.drv_pwr_get_power_ready_st  CVWL668.lib(drv_pwr.o)
    0x0001407c   0x0001407c   0x00000028   Code   RO         1382    i.drv_pwr_set_breath_screen_power_sel  CVWL668.lib(drv_pwr.o)
    0x000140a4   0x000140a4   0x00000028   Code   RO         1383    i.drv_pwr_set_digit_power_sel  CVWL668.lib(drv_pwr.o)
    0x000140cc   0x000140cc   0x00000034   Code   RO         1386    i.drv_pwr_set_pll_clk  CVWL668.lib(drv_pwr.o)
    0x00014100   0x00014100   0x00000034   Code   RO         1387    i.drv_pwr_set_pvd   CVWL668.lib(drv_pwr.o)
    0x00014134   0x00014134   0x0000002c   Code   RO         1390    i.drv_pwr_set_wakeup_type  CVWL668.lib(drv_pwr.o)
    0x00014160   0x00014160   0x00000020   Code   RO         1393    i.drv_pwr_write_lock  CVWL668.lib(drv_pwr.o)
    0x00014180   0x00014180   0x00000010   Code   RO         1987    i.drv_rxbr_clear_pkt_buffer  CVWL668.lib(drv_rxbr.o)
    0x00014190   0x00014190   0x0000000c   Code   RO         1988    i.drv_rxbr_clear_status0  CVWL668.lib(drv_rxbr.o)
    0x0001419c   0x0001419c   0x0000005a   Code   RO         1991    i.drv_rxbr_enable_irq  CVWL668.lib(drv_rxbr.o)
    0x000141f6   0x000141f6   0x00000002   PAD
    0x000141f8   0x000141f8   0x0000001c   Code   RO         1992    i.drv_rxbr_frame_drop_cfg  CVWL668.lib(drv_rxbr.o)
    0x00014214   0x00014214   0x00000018   Code   RO         1001    i.drv_rxbr_get_int_source  CVWL668.lib(hal_internal_vsync.o)
    0x0001422c   0x0001422c   0x00000018   Code   RO         1067    i.drv_rxbr_get_status0  CVWL668.lib(hal_internal_dcs.o)
    0x00014244   0x00014244   0x00000014   Code   RO         2002    i.drv_rxbr_hline_rcv1_cfg  CVWL668.lib(drv_rxbr.o)
    0x00014258   0x00014258   0x00000010   Code   RO         2003    i.drv_rxbr_hline_rcv_cfg  CVWL668.lib(drv_rxbr.o)
    0x00014268   0x00014268   0x0000000c   Code   RO         2005    i.drv_rxbr_register_irq1_callback  CVWL668.lib(drv_rxbr.o)
    0x00014274   0x00014274   0x00000144   Code   RO         2009    i.drv_rxbr_set_cmd_response  CVWL668.lib(drv_rxbr.o)
    0x000143b8   0x000143b8   0x0000001c   Code   RO         2011    i.drv_rxbr_set_color_format  CVWL668.lib(drv_rxbr.o)
    0x000143d4   0x000143d4   0x00000024   Code   RO         2014    i.drv_rxbr_set_filter_regs  CVWL668.lib(drv_rxbr.o)
    0x000143f8   0x000143f8   0x0000001c   Code   RO         2015    i.drv_rxbr_set_inten  CVWL668.lib(drv_rxbr.o)
    0x00014414   0x00014414   0x00000018   Code   RO         2016    i.drv_rxbr_set_ltpo_drop_th  CVWL668.lib(drv_rxbr.o)
    0x0001442c   0x0001442c   0x00000040   Code   RO         2020    i.drv_rxbr_set_usr_cfg  CVWL668.lib(drv_rxbr.o)
    0x0001446c   0x0001446c   0x00000010   Code   RO         2021    i.drv_rxbr_set_usr_col  CVWL668.lib(drv_rxbr.o)
    0x0001447c   0x0001447c   0x00000010   Code   RO         2022    i.drv_rxbr_set_usr_row  CVWL668.lib(drv_rxbr.o)
    0x0001448c   0x0001448c   0x00000078   Code   RO         1644    i.drv_se_init       CVWL668.lib(drv_se.o)
    0x00014504   0x00014504   0x000000d4   Code   RO         1645    i.drv_se_set_dsc    CVWL668.lib(drv_se.o)
    0x000145d8   0x000145d8   0x00000088   Code   RO         1646    i.drv_se_set_lcdc   CVWL668.lib(drv_se.o)
    0x00014660   0x00014660   0x00000090   Code   RO         1647    i.drv_se_set_memc   CVWL668.lib(drv_se.o)
    0x000146f0   0x000146f0   0x000000d0   Code   RO         1648    i.drv_se_set_rxbr   CVWL668.lib(drv_se.o)
    0x000147c0   0x000147c0   0x000000ac   Code   RO         1649    i.drv_se_set_vidc   CVWL668.lib(drv_se.o)
    0x0001486c   0x0001486c   0x00000014   Code   RO         1650    i.drv_se_start_rx   CVWL668.lib(drv_se.o)
    0x00014880   0x00014880   0x0000000c   Code   RO         1456    i.drv_spim_clear_int_status  CVWL668.lib(drv_spi_master.o)
    0x0001488c   0x0001488c   0x00000030   Code   RO         1457    i.drv_spim_disable_int  CVWL668.lib(drv_spi_master.o)
    0x000148bc   0x000148bc   0x0000001c   Code   RO         1461    i.drv_spim_set_inten  CVWL668.lib(drv_spi_master.o)
    0x000148d8   0x000148d8   0x0000001c   Code   RO         1475    i.drv_swire_enable  CVWL668.lib(drv_swire.o)
    0x000148f4   0x000148f4   0x0000000c   Code   RO         1476    i.drv_swire_get_pulse_count  CVWL668.lib(drv_swire.o)
    0x00014900   0x00014900   0x0000000c   Code   RO         1477    i.drv_swire_register_callback  CVWL668.lib(drv_swire.o)
    0x0001490c   0x0001490c   0x00000018   Code   RO         1478    i.drv_swire_set_bit_time  CVWL668.lib(drv_swire.o)
    0x00014924   0x00014924   0x00000048   Code   RO         1479    i.drv_swire_set_int  CVWL668.lib(drv_swire.o)
    0x0001496c   0x0001496c   0x0000001c   Code   RO         1480    i.drv_swire_set_power_down  CVWL668.lib(drv_swire.o)
    0x00014988   0x00014988   0x0000000c   Code   RO         1481    i.drv_swire_set_pulse_count  CVWL668.lib(drv_swire.o)
    0x00014994   0x00014994   0x0000001c   Code   RO         1482    i.drv_swire_set_trig_mode  CVWL668.lib(drv_swire.o)
    0x000149b0   0x000149b0   0x0000000c   Code   RO         1497    i.drv_sys_cfg_clear_all_int  CVWL668.lib(drv_sys_cfg.o)
    0x000149bc   0x000149bc   0x00000028   Code   RO         1498    i.drv_sys_cfg_clear_pending  CVWL668.lib(drv_sys_cfg.o)
    0x000149e4   0x000149e4   0x00000024   Code   RO         1499    i.drv_sys_cfg_sel_ap_rst_trig  CVWL668.lib(drv_sys_cfg.o)
    0x00014a08   0x00014a08   0x00000024   Code   RO         1501    i.drv_sys_cfg_sel_gpio_group  CVWL668.lib(drv_sys_cfg.o)
    0x00014a2c   0x00014a2c   0x00000024   Code   RO         1502    i.drv_sys_cfg_sel_int_trig  CVWL668.lib(drv_sys_cfg.o)
    0x00014a50   0x00014a50   0x00000018   Code   RO         1503    i.drv_sys_cfg_sel_swire_timer  CVWL668.lib(drv_sys_cfg.o)
    0x00014a68   0x00014a68   0x00000024   Code   RO         1504    i.drv_sys_cfg_set_int  CVWL668.lib(drv_sys_cfg.o)
    0x00014a8c   0x00014a8c   0x0000001a   Code   RO         1521    i.drv_timer_clear_status_flags  CVWL668.lib(drv_timer.o)
    0x00014aa6   0x00014aa6   0x00000020   Code   RO         1522    i.drv_timer_enable  CVWL668.lib(drv_timer.o)
    0x00014ac6   0x00014ac6   0x00000002   PAD
    0x00014ac8   0x00014ac8   0x00000010   Code   RO         1523    i.drv_timer_get_instance  CVWL668.lib(drv_timer.o)
    0x00014ad8   0x00014ad8   0x0000003c   Code   RO         1525    i.drv_timer_handle_interrupt  CVWL668.lib(drv_timer.o)
    0x00014b14   0x00014b14   0x00000040   Code   RO         1527    i.drv_timer_set_compare_val  CVWL668.lib(drv_timer.o)
    0x00014b54   0x00014b54   0x00000048   Code   RO         1528    i.drv_timer_set_int  CVWL668.lib(drv_timer.o)
    0x00014b9c   0x00014b9c   0x00000028   Code   RO         1529    i.drv_timer_set_prescaler  CVWL668.lib(drv_timer.o)
    0x00014bc4   0x00014bc4   0x00000010   Code   RO         1530    i.drv_timer_set_repeat  CVWL668.lib(drv_timer.o)
    0x00014bd4   0x00014bd4   0x00000020   Code   RO         1770    i.drv_tx_phy_test_enter  CVWL668.lib(drv_dsi_tx.o)
    0x00014bf4   0x00014bf4   0x00000020   Code   RO         1771    i.drv_tx_phy_test_exit  CVWL668.lib(drv_dsi_tx.o)
    0x00014c14   0x00014c14   0x00000028   Code   RO         1774    i.drv_tx_phy_test_write_code  CVWL668.lib(drv_dsi_tx.o)
    0x00014c3c   0x00014c3c   0x00000034   Code   RO         2159    i.drv_uart_abort_recv  CVWL668.lib(drv_uart.o)
    0x00014c70   0x00014c70   0x00000034   Code   RO         2160    i.drv_uart_abort_send  CVWL668.lib(drv_uart.o)
    0x00014ca4   0x00014ca4   0x00000014   Code   RO         2161    i.drv_uart_config_int  CVWL668.lib(drv_uart.o)
    0x00014cb8   0x00014cb8   0x00000018   Code   RO         2163    i.drv_uart_enable_clk  CVWL668.lib(drv_uart.o)
    0x00014cd0   0x00014cd0   0x0000005c   Code   RO         2164    i.drv_uart_enable_int  CVWL668.lib(drv_uart.o)
    0x00014d2c   0x00014d2c   0x00000028   Code   RO         2166    i.drv_uart_get_instance  CVWL668.lib(drv_uart.o)
    0x00014d54   0x00014d54   0x000000ce   Code   RO         2167    i.drv_uart_init     CVWL668.lib(drv_uart.o)
    0x00014e22   0x00014e22   0x00000002   PAD
    0x00014e24   0x00014e24   0x0000003c   Code   RO         2168    i.drv_uart_int_trans_handle  CVWL668.lib(drv_uart.o)
    0x00014e60   0x00014e60   0x0000001c   Code   RO         2171    i.drv_uart_reset_rx_fifo  CVWL668.lib(drv_uart.o)
    0x00014e7c   0x00014e7c   0x0000001c   Code   RO         2172    i.drv_uart_reset_tx_fifo  CVWL668.lib(drv_uart.o)
    0x00014e98   0x00014e98   0x0000001a   Code   RO         2173    i.drv_uart_send_blocking  CVWL668.lib(drv_uart.o)
    0x00014eb2   0x00014eb2   0x00000054   Code   RO         2175    i.drv_uart_set_baud_rate  CVWL668.lib(drv_uart.o)
    0x00014f06   0x00014f06   0x00000002   PAD
    0x00014f08   0x00014f08   0x0000004c   Code   RO         2176    i.drv_uart_trans_create_handle  CVWL668.lib(drv_uart.o)
    0x00014f54   0x00014f54   0x00000010   Code   RO         2074    i.drv_vidc_clear_irq  CVWL668.lib(drv_vidc.o)
    0x00014f64   0x00014f64   0x00000020   Code   RO         2078    i.drv_vidc_enable   CVWL668.lib(drv_vidc.o)
    0x00014f84   0x00014f84   0x00000040   Code   RO         2079    i.drv_vidc_enable_irq  CVWL668.lib(drv_vidc.o)
    0x00014fc4   0x00014fc4   0x0000002c   Code   RO         2080    i.drv_vidc_get_int_source  CVWL668.lib(drv_vidc.o)
    0x00014ff0   0x00014ff0   0x00000018   Code   RO         2081    i.drv_vidc_get_irq_status  CVWL668.lib(drv_vidc.o)
    0x00015008   0x00015008   0x0000002c   Code   RO         2085    i.drv_vidc_init_module_enable  CVWL668.lib(drv_vidc.o)
    0x00015034   0x00015034   0x0000000c   Code   RO         2086    i.drv_vidc_register_callback  CVWL668.lib(drv_vidc.o)
    0x00015040   0x00015040   0x0000000c   Code   RO         2087    i.drv_vidc_reset    CVWL668.lib(drv_vidc.o)
    0x0001504c   0x0001504c   0x0000001c   Code   RO         2088    i.drv_vidc_set_circ_mode_enable  CVWL668.lib(drv_vidc.o)
    0x00015068   0x00015068   0x00000038   Code   RO         2089    i.drv_vidc_set_dither_config  CVWL668.lib(drv_vidc.o)
    0x000150a0   0x000150a0   0x0000005c   Code   RO         2091    i.drv_vidc_set_dst_parameter  CVWL668.lib(drv_vidc.o)
    0x000150fc   0x000150fc   0x0000000c   Code   RO         2093    i.drv_vidc_set_honly_hcoef0  CVWL668.lib(drv_vidc.o)
    0x00015108   0x00015108   0x0000002c   Code   RO         2094    i.drv_vidc_set_honly_hinitb  CVWL668.lib(drv_vidc.o)
    0x00015134   0x00015134   0x00000030   Code   RO         2095    i.drv_vidc_set_honly_hinitr  CVWL668.lib(drv_vidc.o)
    0x00015164   0x00015164   0x0000001c   Code   RO         2098    i.drv_vidc_set_irqen  CVWL668.lib(drv_vidc.o)
    0x00015180   0x00015180   0x00000014   Code   RO         2099    i.drv_vidc_set_mirror  CVWL668.lib(drv_vidc.o)
    0x00015194   0x00015194   0x0000001c   Code   RO         2102    i.drv_vidc_set_pentile_swap  CVWL668.lib(drv_vidc.o)
    0x000151b0   0x000151b0   0x0000000c   Code   RO         2103    i.drv_vidc_set_pu_ctrl  CVWL668.lib(drv_vidc.o)
    0x000151bc   0x000151bc   0x00000018   Code   RO         2104    i.drv_vidc_set_rotation  CVWL668.lib(drv_vidc.o)
    0x000151d4   0x000151d4   0x0000000c   Code   RO         2105    i.drv_vidc_set_scld_hcoef0  CVWL668.lib(drv_vidc.o)
    0x000151e0   0x000151e0   0x0000000c   Code   RO         2106    i.drv_vidc_set_scld_hcoef1  CVWL668.lib(drv_vidc.o)
    0x000151ec   0x000151ec   0x00000014   Code   RO         2107    i.drv_vidc_set_scld_step  CVWL668.lib(drv_vidc.o)
    0x00015200   0x00015200   0x0000000c   Code   RO         2108    i.drv_vidc_set_scld_vcoef0  CVWL668.lib(drv_vidc.o)
    0x0001520c   0x0001520c   0x0000000c   Code   RO         2109    i.drv_vidc_set_scld_vcoef1  CVWL668.lib(drv_vidc.o)
    0x00015218   0x00015218   0x00000020   Code   RO         2110    i.drv_vidc_set_src_parameter  CVWL668.lib(drv_vidc.o)
    0x00015238   0x00015238   0x00000038   Code   RO         2111    i.drv_vidc_set_vintp_config  CVWL668.lib(drv_vidc.o)
    0x00015270   0x00015270   0x00000034   Code   RO          951    i.fputc             CVWL668.lib(tau_log.o)
    0x000152a4   0x000152a4   0x00000040   Code   RO         1095    i.ha_intl_fb_check_pu_size  CVWL668.lib(hal_internal_fb.o)
    0x000152e4   0x000152e4   0x00000040   Code   RO          557    i.hal_dsi_rx_ctrl_create_handle  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015324   0x00015324   0x00000040   Code   RO          558    i.hal_dsi_rx_ctrl_dcs_async_handler  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015364   0x00015364   0x00000094   Code   RO          559    i.hal_dsi_rx_ctrl_deinit  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x000153f8   0x000153f8   0x000000ac   Code   RO          565    i.hal_dsi_rx_ctrl_init  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x000154a4   0x000154a4   0x00000100   Code   RO          566    i.hal_dsi_rx_ctrl_init_clk  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x000155a4   0x000155a4   0x00000108   Code   RO          567    i.hal_dsi_rx_ctrl_init_dsi_rx  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x000156ac   0x000156ac   0x0000012c   Code   RO          568    i.hal_dsi_rx_ctrl_init_memc  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x000157d8   0x000157d8   0x00000148   Code   RO          569    i.hal_dsi_rx_ctrl_init_rxbr  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015920   0x00015920   0x00000280   Code   RO          570    i.hal_dsi_rx_ctrl_init_vidc  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015ba0   0x00015ba0   0x00000038   Code   RO          571    i.hal_dsi_rx_ctrl_pre_init_pps  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015bd8   0x00015bd8   0x000000b0   Code   RO          577    i.hal_dsi_rx_ctrl_set_auto_ack  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015c88   0x00015c88   0x00000030   Code   RO          582    i.hal_dsi_rx_ctrl_set_ipi_cfg  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015cb8   0x00015cb8   0x00000030   Code   RO          587    i.hal_dsi_rx_ctrl_start  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015ce8   0x00015ce8   0x00000030   Code   RO          588    i.hal_dsi_rx_ctrl_stop  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015d18   0x00015d18   0x00000020   Code   RO          590    i.hal_dsi_rx_ctrl_toggle_resolution  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015d38   0x00015d38   0x0000027c   Code   RO          637    i.hal_dsi_tx_cmd_mode_cal_timing  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00015fb4   0x00015fb4   0x00000038   Code   RO          639    i.hal_dsi_tx_ctrl_create_handle  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00015fec   0x00015fec   0x00000074   Code   RO          640    i.hal_dsi_tx_ctrl_deinit  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00016060   0x00016060   0x00000022   Code   RO          643    i.hal_dsi_tx_ctrl_gen_a_tear_signal  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00016082   0x00016082   0x00000002   PAD
    0x00016084   0x00016084   0x0000007c   Code   RO          645    i.hal_dsi_tx_ctrl_init  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00016100   0x00016100   0x00000010   Code   RO          646    i.hal_dsi_tx_ctrl_init_clk  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00016110   0x00016110   0x00000008   Code   RO          659    i.hal_dsi_tx_ctrl_set_overwrite_rgb  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00016118   0x00016118   0x0000000a   Code   RO          660    i.hal_dsi_tx_ctrl_set_tear_mode  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00016122   0x00016122   0x00000002   PAD
    0x00016124   0x00016124   0x00000090   Code   RO          662    i.hal_dsi_tx_ctrl_start  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000161b4   0x000161b4   0x00000038   Code   RO          663    i.hal_dsi_tx_ctrl_stop  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000161ec   0x000161ec   0x000000f4   Code   RO          665    i.hal_dsi_tx_ctrl_write_array_cmd  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000162e0   0x000162e0   0x000000d0   Code   RO          666    i.hal_dsi_tx_ctrl_write_cmd  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000163b0   0x000163b0   0x00000104   Code   RO          667    i.hal_dsi_tx_init_cfg  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000164b4   0x000164b4   0x00000044   Code   RO          668    i.hal_dsi_tx_init_dpi_timing  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000164f8   0x000164f8   0x00000016   Code   RO          669    i.hal_dsi_tx_init_phy_cfg  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x0001650e   0x0001650e   0x00000052   Code   RO          670    i.hal_dsi_tx_init_timing  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00016560   0x00016560   0x00000054   Code   RO          671    i.hal_dsi_tx_init_vid_timing  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000165b4   0x000165b4   0x00000040   Code   RO          672    i.hal_dsi_tx_send_cmd  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000165f4   0x000165f4   0x00000094   Code   RO          673    i.hal_dsi_tx_timing_info_update  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00016688   0x00016688   0x00000310   Code   RO          674    i.hal_dsi_tx_vid_mode_cal_timing  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00016998   0x00016998   0x0000003a   Code   RO          744    i.hal_gpio_config_pad  CVWL668.lib(hal_gpio.o)
    0x000169d2   0x000169d2   0x00000002   PAD
    0x000169d4   0x000169d4   0x00000018   Code   RO          745    i.hal_gpio_ctrl_eint  CVWL668.lib(hal_gpio.o)
    0x000169ec   0x000169ec   0x00000012   Code   RO          746    i.hal_gpio_get_input_data  CVWL668.lib(hal_gpio.o)
    0x000169fe   0x000169fe   0x00000002   PAD
    0x00016a00   0x00016a00   0x00000040   Code   RO          749    i.hal_gpio_init_eint  CVWL668.lib(hal_gpio.o)
    0x00016a40   0x00016a40   0x00000016   Code   RO          750    i.hal_gpio_init_input  CVWL668.lib(hal_gpio.o)
    0x00016a56   0x00016a56   0x0000001c   Code   RO          751    i.hal_gpio_init_output  CVWL668.lib(hal_gpio.o)
    0x00016a72   0x00016a72   0x00000002   PAD
    0x00016a74   0x00016a74   0x0000001c   Code   RO          752    i.hal_gpio_reg_eint_cb  CVWL668.lib(hal_gpio.o)
    0x00016a90   0x00016a90   0x00000050   Code   RO          753    i.hal_gpio_set_ap_reset_int  CVWL668.lib(hal_gpio.o)
    0x00016ae0   0x00016ae0   0x00000060   Code   RO          756    i.hal_gpio_set_mode  CVWL668.lib(hal_gpio.o)
    0x00016b40   0x00016b40   0x00000008   Code   RO          757    i.hal_gpio_set_output_data  CVWL668.lib(hal_gpio.o)
    0x00016b48   0x00016b48   0x00000048   Code   RO          758    i.hal_gpio_set_pull_state  CVWL668.lib(hal_gpio.o)
    0x00016b90   0x00016b90   0x00000010   Code   RO         1003    i.hal_internal_sync_get_hight_performan_mode  CVWL668.lib(hal_internal_vsync.o)
    0x00016ba0   0x00016ba0   0x000001b4   Code   RO         1004    i.hal_internal_sync_input_resolution_change  CVWL668.lib(hal_internal_vsync.o)
    0x00016d54   0x00016d54   0x0000000c   Code   RO         1005    i.hal_internal_sync_register_lcdc_cb  CVWL668.lib(hal_internal_vsync.o)
    0x00016d60   0x00016d60   0x00000020   Code   RO         1008    i.hal_internal_vsync_deinit  CVWL668.lib(hal_internal_vsync.o)
    0x00016d80   0x00016d80   0x0000000c   Code   RO         1009    i.hal_internal_vsync_get_rx_state  CVWL668.lib(hal_internal_vsync.o)
    0x00016d8c   0x00016d8c   0x00000014   Code   RO         1010    i.hal_internal_vsync_get_sync_line  CVWL668.lib(hal_internal_vsync.o)
    0x00016da0   0x00016da0   0x0000000c   Code   RO         1011    i.hal_internal_vsync_get_tx_state  CVWL668.lib(hal_internal_vsync.o)
    0x00016dac   0x00016dac   0x000000e8   Code   RO         1012    i.hal_internal_vsync_init_rx  CVWL668.lib(hal_internal_vsync.o)
    0x00016e94   0x00016e94   0x000000c8   Code   RO         1013    i.hal_internal_vsync_init_tx  CVWL668.lib(hal_internal_vsync.o)
    0x00016f5c   0x00016f5c   0x00000020   Code   RO         1014    i.hal_internal_vsync_set_rx_state  CVWL668.lib(hal_internal_vsync.o)
    0x00016f7c   0x00016f7c   0x0000013c   Code   RO         1016    i.hal_internal_vsync_set_tear_mode  CVWL668.lib(hal_internal_vsync.o)
    0x000170b8   0x000170b8   0x00000058   Code   RO         1017    i.hal_internal_vsync_set_tx_state  CVWL668.lib(hal_internal_vsync.o)
    0x00017110   0x00017110   0x0000006c   Code   RO         1068    i.hal_intl_dcs_init_sw_fltr  CVWL668.lib(hal_internal_dcs.o)
    0x0001717c   0x0001717c   0x0000044c   Code   RO         1070    i.hal_intl_dcs_rx_get_dcs_packet_data  CVWL668.lib(hal_internal_dcs.o)
    0x000175c8   0x000175c8   0x00000088   Code   RO         1071    i.hal_intl_dcs_rx_receive_packet  CVWL668.lib(hal_internal_dcs.o)
    0x00017650   0x00017650   0x00000174   Code   RO         1072    i.hal_intl_dcs_rx_receive_pps  CVWL668.lib(hal_internal_dcs.o)
    0x000177c4   0x000177c4   0x0000008c   Code   RO         1073    i.hal_intl_dcs_set_auto_hw_filter  CVWL668.lib(hal_internal_dcs.o)
    0x00017850   0x00017850   0x0000002c   Code   RO         1075    i.hal_intl_dcs_sw_filter_handle  CVWL668.lib(hal_internal_dcs.o)
    0x0001787c   0x0001787c   0x000002f0   Code   RO         1096    i.hal_intl_fb_cal_fb_info  CVWL668.lib(hal_internal_fb.o)
    0x00017b6c   0x00017b6c   0x00000064   Code   RO         1097    i.hal_intl_fb_check_bandwidth  CVWL668.lib(hal_internal_fb.o)
    0x00017bd0   0x00017bd0   0x000000dc   Code   RO         1098    i.hal_intl_fb_edge_resize  CVWL668.lib(hal_internal_fb.o)
    0x00017cac   0x00017cac   0x00000074   Code   RO         1099    i.hal_intl_fb_flow_control_adapter  CVWL668.lib(hal_internal_fb.o)
    0x00017d20   0x00017d20   0x0000000c   Code   RO         1100    i.hal_intl_fb_get_memc_flow_mode  CVWL668.lib(hal_internal_fb.o)
    0x00017d2c   0x00017d2c   0x00000010   Code   RO         1101    i.hal_intl_fb_get_rx_fb_info  CVWL668.lib(hal_internal_fb.o)
    0x00017d3c   0x00017d3c   0x00000010   Code   RO         1102    i.hal_intl_fb_get_tx_fb_info  CVWL668.lib(hal_internal_fb.o)
    0x00017d4c   0x00017d4c   0x0000000c   Code   RO         1103    i.hal_intl_fb_get_user_flow  CVWL668.lib(hal_internal_fb.o)
    0x00017d58   0x00017d58   0x00000028   Code   RO         1121    i.hal_intl_svs_deinit_rx  CVWL668.lib(hal_internal_svs.o)
    0x00017d80   0x00017d80   0x00000010   Code   RO         1122    i.hal_intl_svs_deinit_tx  CVWL668.lib(hal_internal_svs.o)
    0x00017d90   0x00017d90   0x00000024   Code   RO         1123    i.hal_intl_svs_handle  CVWL668.lib(hal_internal_svs.o)
    0x00017db4   0x00017db4   0x00000080   Code   RO         1124    i.hal_intl_svs_init_rx  CVWL668.lib(hal_internal_svs.o)
    0x00017e34   0x00017e34   0x00000014   Code   RO         1125    i.hal_intl_svs_init_tx  CVWL668.lib(hal_internal_svs.o)
    0x00017e48   0x00017e48   0x0000000c   Code   RO         1127    i.hal_intl_svs_set_rx_vtt  CVWL668.lib(hal_internal_svs.o)
    0x00017e54   0x00017e54   0x00000048   Code   RO         1129    i.hal_intl_svs_update_rxbr_clk  CVWL668.lib(hal_internal_svs.o)
    0x00017e9c   0x00017e9c   0x00000070   Code   RO          675    i.hal_lcdc_displayproc_config  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00017f0c   0x00017f0c   0x0000003e   Code   RO          676    i.hal_lcdc_init_cfg  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00017f4a   0x00017f4a   0x00000070   Code   RO          677    i.hal_lcdc_init_clk  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00017fba   0x00017fba   0x00000002   PAD
    0x00017fbc   0x00017fbc   0x00000128   Code   RO          678    i.hal_lcdc_postproc_config  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000180e4   0x000180e4   0x00000024   Code   RO          679    i.hal_lcdc_start    CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00018108   0x00018108   0x0000003c   Code   RO          680    i.hal_lcdc_timinggen_config  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00018144   0x00018144   0x000000e0   Code   RO          681    i.hal_lcdc_upscaler_config  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00018224   0x00018224   0x000000bc   Code   RO          683    i.hal_nonshadow_func_update  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000182e0   0x000182e0   0x0000002a   Code   RO          902    i.hal_pwr_enter_deep_sleep_mode  CVWL668.lib(hal_pwr.o)
    0x0001830a   0x0001830a   0x00000008   Code   RO          903    i.hal_pwr_enter_normal_sleep_mode  CVWL668.lib(hal_pwr.o)
    0x00018312   0x00018312   0x00000002   PAD
    0x00018314   0x00018314   0x00000064   Code   RO          904    i.hal_pwr_enter_stop_sleep_mode  CVWL668.lib(hal_pwr.o)
    0x00018378   0x00018378   0x0000000a   Code   RO          905    i.hal_pwr_exit_sleep_mode  CVWL668.lib(hal_pwr.o)
    0x00018382   0x00018382   0x00000008   Code   RO          907    i.hal_pwr_get_vcc_power_ready  CVWL668.lib(hal_pwr.o)
    0x0001838a   0x0001838a   0x00000008   Code   RO          912    i.hal_pwr_set_main_power  CVWL668.lib(hal_pwr.o)
    0x00018392   0x00018392   0x00000008   Code   RO          913    i.hal_pwr_set_pvd   CVWL668.lib(hal_pwr.o)
    0x0001839a   0x0001839a   0x00000008   Code   RO          914    i.hal_pwr_set_sleep_mode_power  CVWL668.lib(hal_pwr.o)
    0x000183a2   0x000183a2   0x00000002   PAD
    0x000183a4   0x000183a4   0x00000064   Code   RO          915    i.hal_pwr_set_stop_sleep_wakeup_pin  CVWL668.lib(hal_pwr.o)
    0x00018408   0x00018408   0x00000040   Code   RO          838    i.hal_swire_deinit  CVWL668.lib(hal_swire.o)
    0x00018448   0x00018448   0x0000005c   Code   RO          839    i.hal_swire_enable  CVWL668.lib(hal_swire.o)
    0x000184a4   0x000184a4   0x00000058   Code   RO          840    i.hal_swire_init    CVWL668.lib(hal_swire.o)
    0x000184fc   0x000184fc   0x00000024   Code   RO          842    i.hal_swire_set_pulse  CVWL668.lib(hal_swire.o)
    0x00018520   0x00018520   0x00000040   Code   RO          843    i.hal_swire_set_timer  CVWL668.lib(hal_swire.o)
    0x00018560   0x00018560   0x00000008   Code   RO          859    i.hal_system_enable_systick  CVWL668.lib(hal_system.o)
    0x00018568   0x00018568   0x00000008   Code   RO          861    i.hal_system_get_tick  CVWL668.lib(hal_system.o)
    0x00018570   0x00018570   0x000000e4   Code   RO          863    i.hal_system_init   CVWL668.lib(hal_system.o)
    0x00018654   0x00018654   0x00000050   Code   RO          866    i.hal_system_updata_sysclk  CVWL668.lib(hal_system.o)
    0x000186a4   0x000186a4   0x00000030   Code   RO          881    i.hal_timer_deinit  CVWL668.lib(hal_timer.o)
    0x000186d4   0x000186d4   0x0000001c   Code   RO          883    i.hal_timer_init    CVWL668.lib(hal_timer.o)
    0x000186f0   0x000186f0   0x00000008   Code   RO          884    i.hal_timer_set_repeat  CVWL668.lib(hal_timer.o)
    0x000186f8   0x000186f8   0x00000030   Code   RO          684    i.hal_tx_frame_rate_adjust  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00018728   0x00018728   0x00000094   Code   RO          975    i.hal_uart_init     CVWL668.lib(hal_uart.o)
    0x000187bc   0x000187bc   0x0000001c   Code   RO          978    i.hal_uart_send_blocking  CVWL668.lib(hal_uart.o)
    0x000187d8   0x000187d8   0x00000018   Code   RO          685    i.hal_vsync_func_update  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000187f0   0x000187f0   0x000000e0   Code   RO         1019    i.hal_vsync_reset_lcdc_scaler  CVWL668.lib(hal_internal_vsync.o)
    0x000188d0   0x000188d0   0x00000040   Code   RO            3    i.main              main.o
    0x00018910   0x00018910   0x00000054   Code   RO          346    i.pps_update_handle  s8_demo.o
    0x00018964   0x00018964   0x000002e4   Code   RO         1020    i.rxbr_irq1_callback  CVWL668.lib(hal_internal_vsync.o)
    0x00018c48   0x00018c48   0x00000064   Code   RO          347    i.s8_demo           s8_demo.o
    0x00018cac   0x00018cac   0x0000003a   Code   RO          348    i.send_panel_init_code  s8_demo.o
    0x00018ce6   0x00018ce6   0x00000002   PAD
    0x00018ce8   0x00018ce8   0x00000044   Code   RO         1021    i.soft_double_buffer_update  CVWL668.lib(hal_internal_vsync.o)
    0x00018d2c   0x00018d2c   0x0000006c   Code   RO         1022    i.soft_gen_te       CVWL668.lib(hal_internal_vsync.o)
    0x00018d98   0x00018d98   0x000000e0   Code   RO         1023    i.soft_gen_te_double_buffer  CVWL668.lib(hal_internal_vsync.o)
    0x00018e78   0x00018e78   0x00000038   Code   RO         1024    i.soft_pro_motion_init  CVWL668.lib(hal_internal_vsync.o)
    0x00018eb0   0x00018eb0   0x00000024   Code   RO         1025    i.soft_tear_adjust_line  CVWL668.lib(hal_internal_vsync.o)
    0x00018ed4   0x00018ed4   0x00000018   Code   RO          917    i.stop_sleep_cb     CVWL668.lib(hal_pwr.o)
    0x00018eec   0x00018eec   0x000000ac   Code   RO         1130    i.svs_direct_mode_setting  CVWL668.lib(hal_internal_svs.o)
    0x00018f98   0x00018f98   0x0000001c   Code   RO         1131    i.svs_get_rel_intv  CVWL668.lib(hal_internal_svs.o)
    0x00018fb4   0x00018fb4   0x000000b0   Code   RO         1132    i.svs_sync_handle   CVWL668.lib(hal_internal_svs.o)
    0x00019064   0x00019064   0x000000cc   Code   RO         1133    i.svs_wait_fr_stab  CVWL668.lib(hal_internal_svs.o)
    0x00019130   0x00019130   0x0000010c   Code   RO         1134    i.svs_wait_start    CVWL668.lib(hal_internal_svs.o)
    0x0001923c   0x0001923c   0x00000034   Code   RO          952    i.tau_log_init      CVWL668.lib(tau_log.o)
    0x00019270   0x00019270   0x00000084   Code   RO          953    i.tau_log_printf    CVWL668.lib(tau_log.o)
    0x000192f4   0x000192f4   0x00000076   Code   RO          954    i.tau_log_push_log  CVWL668.lib(tau_log.o)
    0x0001936a   0x0001936a   0x00000002   PAD
    0x0001936c   0x0001936c   0x000000b4   Code   RO         1026    i.vidc_callback     CVWL668.lib(hal_internal_vsync.o)
    0x00019420   0x00019420   0x00000118   Code   RO         1027    i.vpre_err_reset    CVWL668.lib(hal_internal_vsync.o)
    0x00019538   0x00019538   0x00001f08   Data   RO          352    .constdata          s8_demo.o
    0x0001b440   0x0001b440   0x00000028   Data   RO          592    .constdata          CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x0001b468   0x0001b468   0x0000001c   Data   RO          688    .constdata          CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x0001b484   0x0001b484   0x000000b6   Data   RO          761    .constdata          CVWL668.lib(hal_gpio.o)
    0x0001b53a   0x0001b53a   0x00000002   PAD
    0x0001b53c   0x0001b53c   0x00000030   Data   RO          980    .constdata          CVWL668.lib(hal_uart.o)
    0x0001b56c   0x0001b56c   0x00000010   Data   RO         2178    .constdata          CVWL668.lib(drv_uart.o)
    0x0001b57c   0x0001b57c   0x00000087   Data   RO          593    .conststring        CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x0001b603   0x0001b603   0x00000001   PAD
    0x0001b604   0x0001b604   0x00000090   Data   RO         1029    .conststring        CVWL668.lib(hal_internal_vsync.o)
    0x0001b694   0x0001b694   0x0000008e   Data   RO         1078    .conststring        CVWL668.lib(hal_internal_dcs.o)
    0x0001b722   0x0001b722   0x00000002   PAD
    0x0001b724   0x0001b724   0x00000020   Data   RO         2580    Region$$Table       anon$$obj.o


    Execution Region RW_IRAM1 (Exec base: 0x00070000, Load base: 0x0001b744, Size: 0x00003118, Max: 0x00008000, ABSOLUTE, COMPRESSED[0x00000160])

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00070000   COMPRESSED   0x00000094   Data   RW          353    .data               s8_demo.o
    0x00070094   COMPRESSED   0x00000024   Data   RW          594    .data               CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x000700b8   COMPRESSED   0x0000005c   Data   RW          689    .data               CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00070114   COMPRESSED   0x00000001   Data   RW          824    .data               CVWL668.lib(hal_spi_master.o)
    0x00070115   COMPRESSED   0x00000002   Data   RW          845    .data               CVWL668.lib(hal_swire.o)
    0x00070117   COMPRESSED   0x00000001   PAD
    0x00070118   COMPRESSED   0x00000008   Data   RW          918    .data               CVWL668.lib(hal_pwr.o)
    0x00070120   COMPRESSED   0x00000001   Data   RW          957    .data               CVWL668.lib(tau_log.o)
    0x00070121   COMPRESSED   0x00000003   PAD
    0x00070124   COMPRESSED   0x00000018   Data   RW          981    .data               CVWL668.lib(hal_uart.o)
    0x0007013c   COMPRESSED   0x00000010   Data   RW         1030    .data               CVWL668.lib(hal_internal_vsync.o)
    0x0007014c   COMPRESSED   0x00000024   Data   RW         1079    .data               CVWL668.lib(hal_internal_dcs.o)
    0x00070170   COMPRESSED   0x0000000c   Data   RW         1163    .data               CVWL668.lib(drv_common.o)
    0x0007017c   COMPRESSED   0x00000001   Data   RW         1164    .data               CVWL668.lib(drv_common.o)
    0x0007017d   COMPRESSED   0x00000003   PAD
    0x00070180   COMPRESSED   0x00000190   Data   RW         1249    .data               CVWL668.lib(drv_dma.o)
    0x00070310   COMPRESSED   0x00000004   Data   RW         1313    .data               CVWL668.lib(drv_gpio.o)
    0x00070314   COMPRESSED   0x00000004   Data   RW         1483    .data               CVWL668.lib(drv_swire.o)
    0x00070318   COMPRESSED   0x00000050   Data   RW         1531    .data               CVWL668.lib(drv_timer.o)
    0x00070368   COMPRESSED   0x00000024   Data   RW         1582    .data               CVWL668.lib(drv_i2c.o)
    0x0007038c   COMPRESSED   0x00000004   Data   RW         1651    .data               CVWL668.lib(drv_se.o)
    0x00070390   COMPRESSED   0x00000001   Data   RW         1691    .data               CVWL668.lib(drv_dsi_rx.o)
    0x00070391   COMPRESSED   0x00000003   PAD
    0x00070394   COMPRESSED   0x00000008   Data   RW         2026    .data               CVWL668.lib(drv_rxbr.o)
    0x0007039c   COMPRESSED   0x00000004   Data   RW         2113    .data               CVWL668.lib(drv_vidc.o)
    0x000703a0   COMPRESSED   0x00000004   Data   RW         2558    .data               mc_p.l(stdout.o)
    0x000703a4        -       0x000000d0   Zero   RW          591    .bss                CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00070474        -       0x000000b8   Zero   RW          687    .bss                CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x0007052c        -       0x00000100   Zero   RW          956    .bss                CVWL668.lib(tau_log.o)
    0x0007062c        -       0x00000044   Zero   RW         1028    .bss                CVWL668.lib(hal_internal_vsync.o)
    0x00070670        -       0x00000800   Zero   RW         1076    .bss                CVWL668.lib(hal_internal_dcs.o)
    0x00070e70        -       0x000000ff   Zero   RW         1077    .bss                CVWL668.lib(hal_internal_dcs.o)
    0x00070f6f   COMPRESSED   0x00000001   PAD
    0x00070f70        -       0x00000044   Zero   RW         1105    .bss                CVWL668.lib(hal_internal_fb.o)
    0x00070fb4        -       0x00000044   Zero   RW         1135    .bss                CVWL668.lib(hal_internal_svs.o)
    0x00070ff8        -       0x00000010   Zero   RW         1247    .bss                CVWL668.lib(drv_dma.o)
    0x00071008        -       0x00000040   Zero   RW         1312    .bss                CVWL668.lib(drv_gpio.o)
    0x00071048        -       0x0000106c   Zero   RW         1634    .bss                CVWL668.lib(dcs_packet_fifo.o)
    0x000720b4        -       0x00000060   Zero   RW         2177    .bss                CVWL668.lib(drv_uart.o)
    0x00072114   COMPRESSED   0x00000004   PAD
    0x00072118        -       0x00001000   Zero   RW          546    STACK               startup_armcm0.o


==============================================================================

Image component sizes


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Object Name

         0          0          0          0          0       5336   app_tp_transfer.o
        32          6          0          0          0        585   board.o
        64         32          0          0          0      10483   main.o
      2490        546       7944        148          0      26985   s8_demo.o
       120         18        192          0       4096       2148   startup_armcm0.o

    ----------------------------------------------------------------------
      2712        602       8168        148       4096      45537   Object Totals
         0          0         32          0          0          0   (incl. Generated)
         6          0          0          0          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Member Name

       216         32          0          0       4204        252   dcs_packet_fifo.o
       204         86         28         13          0        324   drv_common.o
       536         90          0          0          0        792   drv_crgu.o
       136         22          0        400         16        196   drv_dma.o
       144         34          0          0          0        248   drv_dsc_dec.o
      1892        678          0          1          0       1280   drv_dsi_rx.o
      1704        306          0          0          0       2036   drv_dsi_tx.o
       148          0          0          0          0        260   drv_efuse.o
       364         54          0          4         64       1192   drv_gpio.o
        36         12          0         36          0        180   drv_i2c.o
      1080        166          0          0          0       1620   drv_lcdc.o
       658        104          0          0          0       1240   drv_memc.o
        40          0          0          0          0        120   drv_phy_common.o
       644        144          0          0          0        784   drv_pwr.o
       814        110          0          8          0       1136   drv_rxbr.o
      1012        264          0          4          0        492   drv_se.o
        88         20          0          0          0        188   drv_spi_master.o
       264         54          0          4          0        560   drv_swire.o
       220         40          0          0          0        428   drv_sys_cfg.o
       366         38          0         80          0        816   drv_timer.o
      1172         54         16          0         96        980   drv_uart.o
       824        152          0          4          0       1700   drv_vidc.o
      2670        198        175         36        208       1168   hal_dsi_rx_ctrl.o
      4326        338         50         92        184       2212   hal_dsi_tx_ctrl.o
       530         38        182          0          0        828   hal_gpio.o
      2168        510        142         36       2303        652   hal_internal_dcs.o
      1308         60          0          0         68        700   hal_internal_fb.o
      1172        182          0          0         68        840   hal_internal_svs.o
      3648        754        144         16         68       1688   hal_internal_vsync.o
       316         32          0          8          0        684   hal_pwr.o
        72         10          0          1          0         68   hal_spi_master.o
       344         32          0          2          0        348   hal_swire.o
       324         56          0          0          0        272   hal_system.o
        84          0          0          0          0        204   hal_timer.o
       176         18         48         24          0        144   hal_uart.o
        68          4          0          0          0        136   tau_delay.o
       354         30         16          1        256        320   tau_log.o
       200         20          0          0          0         76   ceil.o
        86          0          0          0          0          0   __dczerorl2.o
         0          0          0          0          0          0   entry.o
         0          0          0          0          0          0   entry10a.o
         0          0          0          0          0          0   entry11a.o
         8          4          0          0          0          0   entry2.o
         4          0          0          0          0          0   entry5.o
         0          0          0          0          0          0   entry7b.o
         0          0          0          0          0          0   entry8b.o
         8          4          0          0          0          0   entry9a.o
        30          0          0          0          0          0   handlers.o
        40          0          0          0          0         72   idiv.o
        36          8          0          0          0         68   init.o
         0          0          0          0          0          0   iusefp.o
        32          0          0          0          0         68   llshl.o
        38          0          0          0          0         68   llsshr.o
        34          0          0          0          0         68   llushr.o
        26          0          0          0          0         72   memcmp.o
        36          0          0          0          0         60   memcpya.o
        36          0          0          0          0        100   memseta.o
      2298        104          0          0          0        544   printfa.o
         0          0          0          4          0          0   stdout.o
        14          0          0          0          0         60   strlen.o
        44          0          0          0          0         72   uidiv.o
        96          0          0          0          0         84   uldiv.o
        40          2          0          0          0         68   cdrcmple.o
        20          0          0          0          0         68   cfcmple.o
        20          0          0          0          0         68   cfrcmple.o
        56          0          0          0          0         68   d2f.o
       356          4          0          0          0        140   dadd.o
       240          6          0          0          0         84   ddiv.o
       236          0          0          0          0        216   depilogue.o
        60         10          0          0          0         68   dfixui.o
        64         10          0          0          0         68   dfixul.o
        28          4          0          0          0         68   dfltui.o
       208          6          0          0          0         88   dmul.o
        40          0          0          0          0         60   f2d.o
       178          0          0          0          0        108   fadd.o
       124          0          0          0          0         72   fdiv.o
       130          0          0          0          0        144   fepilogue.o
        40          0          0          0          0         60   ffixui.o
        14          0          0          0          0         68   ffltui.o
       122          0          0          0          0         72   fmul.o
        24          0          0          0          0         60   fscalb.o

    ----------------------------------------------------------------------
     35228       4904        808        784       7540      30148   Library Totals
        40          0          7         10          5          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Name

     30122       4722        801        770       7535      27088   CVWL668.lib
       200         20          0          0          0         76   m_ps.l
      2866        120          0          4          0       1336   mc_p.l
      2000         42          0          0          0       1648   mf_p.l

    ----------------------------------------------------------------------
     35228       4904        808        784       7540      30148   Library Totals

    ----------------------------------------------------------------------

==============================================================================


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   

     37940       5506       8976        932      11636      55425   Grand Totals
     37940       5506       8976        352      11636      55425   ELF Image Totals (compressed)
     37940       5506       8976        352          0          0   ROM Totals

==============================================================================

    Total RO  Size (Code + RO Data)                46916 (  45.82kB)
    Total RW  Size (RW Data + ZI Data)             12568 (  12.27kB)
    Total ROM Size (Code + RO Data + RW Data)      47268 (  46.16kB)

==============================================================================

