Component: ARM Compiler 5.06 update 6 (build 750) Tool: armlink [4d35ed]

==============================================================================

Section Cross References

    main.o(i.main) refers to board.o(i.board_Init) for board_Init
    main.o(i.main) refers to s8_demo.o(i.s8_demo) for s8_demo
    main.o(i.main) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(i.app_tp_transfer_phone) for app_tp_transfer_phone
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(i.app_tp_s_write) for app_tp_s_write
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(.data) for i2cs_transfer
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(i.app_tp_phone_reset_init) for app_tp_phone_reset_init
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(i.app_tp_screen_int_init) for app_tp_screen_int_init
    app_tp_transfer.o(i.app_tp_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(i.screen_spim_io_init) for screen_spim_io_init
    app_tp_transfer.o(i.app_tp_init) refers to hal_spi_master.o(i.hal_spim_init) for hal_spim_init
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(i.phone_i2cs_io_init) for phone_i2cs_io_init
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_slave.o(i.hal_i2cs_init) for hal_i2cs_init
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_slave.o(i.hal_i2cs_register_callback) for hal_i2cs_register_callback
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) for hal_i2cs_update_rx_buffer
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer) for hal_i2cs_update_tx_buffer
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_slave.o(i.hal_i2cs_start) for hal_i2cs_start
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_for_custom_s8.o(.data) for g_phone_output_int_pad
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(i.app_tp_i2cs_callback) for app_tp_i2cs_callback
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(.bss) for s_phone_read_buffer
    app_tp_transfer.o(i.app_tp_m_read) refers to hal_spi_master.o(i.hal_spim_read) for hal_spim_read
    app_tp_transfer.o(i.app_tp_m_transfer_complate) refers to hal_spi_master.o(i.hal_spim_get_transfer_complete) for hal_spim_get_transfer_complete
    app_tp_transfer.o(i.app_tp_m_write) refers to hal_spi_master.o(i.hal_spim_write) for hal_spim_write
    app_tp_transfer.o(i.app_tp_m_write) refers to app_tp_transfer.o(.data) for s_spim_write
    app_tp_transfer.o(i.app_tp_phone_clear_reset_on) refers to app_tp_transfer.o(.data) for s_phone_reset_flag
    app_tp_transfer.o(i.app_tp_phone_reset_init) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    app_tp_transfer.o(i.app_tp_phone_reset_init) refers to hal_gpio.o(i.hal_gpio_ctrl_eint) for hal_gpio_ctrl_eint
    app_tp_transfer.o(i.app_tp_phone_reset_init) refers to hal_gpio.o(i.hal_gpio_init_eint) for hal_gpio_init_eint
    app_tp_transfer.o(i.app_tp_phone_reset_init) refers to hal_gpio.o(i.hal_gpio_reg_eint_cb) for hal_gpio_reg_eint_cb
    app_tp_transfer.o(i.app_tp_phone_reset_init) refers to app_tp_for_custom_s8.o(.data) for g_phone_input_rst_pad
    app_tp_transfer.o(i.app_tp_phone_reset_init) refers to app_tp_transfer.o(i.app_tp_reset_callback) for app_tp_reset_callback
    app_tp_transfer.o(i.app_tp_phone_reset_on) refers to app_tp_transfer.o(.data) for s_phone_reset_flag
    app_tp_transfer.o(i.app_tp_reset_callback) refers to app_tp_transfer.o(.data) for s_phone_reset_flag
    app_tp_transfer.o(i.app_tp_s_read) refers to hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) for hal_i2cs_update_rx_buffer
    app_tp_transfer.o(i.app_tp_s_write) refers to hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer) for hal_i2cs_update_tx_buffer
    app_tp_transfer.o(i.app_tp_screen_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    app_tp_transfer.o(i.app_tp_screen_init) refers to tau_delay.o(i.delayUs) for delayUs
    app_tp_transfer.o(i.app_tp_screen_init) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_transfer.o(i.app_tp_screen_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_rst_pad
    app_tp_transfer.o(i.app_tp_screen_int_callback) refers to app_tp_transfer.o(.data) for s_screen_int_flag
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to hal_gpio.o(i.hal_gpio_ctrl_eint) for hal_gpio_ctrl_eint
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to hal_gpio.o(i.hal_gpio_init_eint) for hal_gpio_init_eint
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to hal_gpio.o(i.hal_gpio_reg_eint_cb) for hal_gpio_reg_eint_cb
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to app_tp_transfer.o(i.app_tp_screen_int_callback) for app_tp_screen_int_callback
    app_tp_transfer.o(i.app_tp_screen_int_lvl_low) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    app_tp_transfer.o(i.app_tp_screen_int_lvl_low) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.app_tp_transfer_phone) refers to app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) for app_tp_phone_analysis_data
    app_tp_transfer.o(i.app_tp_transfer_phone) refers to app_tp_transfer.o(i.app_tp_s_read) for app_tp_s_read
    app_tp_transfer.o(i.app_tp_transfer_phone) refers to app_tp_transfer.o(.data) for s_slave_txbuffer_size
    app_tp_transfer.o(i.app_tp_transfer_phone) refers to app_tp_transfer.o(.bss) for s_phone_read_buffer
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(i.app_tp_m_transfer_complate) for app_tp_m_transfer_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to hal_spi_master.o(i.hal_spim_flush) for hal_spim_flush
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) for app_tp_screen_analysis_const
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(.data) for s_screen_const_transfer_count
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_for_custom_s8.o(.constdata) for screen_reg_start_data_size
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_for_custom_s8.o(.data) for screen_reg_start_data
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(.bss) for s_screen_read_buffer
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_transfer_screen_const) for app_tp_transfer_screen_const
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_screen_int_lvl_low) for app_tp_screen_int_lvl_low
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_m_transfer_complate) for app_tp_m_transfer_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_spi_master.o(i.hal_spim_flush) for hal_spim_flush
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) for app_tp_screen_analysis_int
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_system.o(i.hal_system_get_tick) for hal_system_get_tick
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(i.app_tp_write_other_operations) for app_tp_write_other_operations
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(.data) for s_screen_init_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(.data) for screen_reg_int_data
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(.bss) for s_screen_read_buffer
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(.constdata) for screen_reg_int_data_size
    app_tp_transfer.o(i.app_tp_transfer_screen_start) refers to app_tp_transfer.o(i.app_tp_screen_init) for app_tp_screen_init
    app_tp_transfer.o(i.app_tp_transfer_screen_start) refers to app_tp_transfer.o(i.app_tp_transfer_screen_const) for app_tp_transfer_screen_const
    app_tp_transfer.o(i.app_tp_transfer_screen_start) refers to app_tp_transfer.o(.data) for s_screen_init_complate
    app_tp_transfer.o(i.phone_i2cs_io_init) refers to hal_gpio.o(i.hal_gpio_config_pad) for hal_gpio_config_pad
    app_tp_transfer.o(i.phone_i2cs_io_init) refers to app_tp_transfer.o(.constdata) for .constdata
    app_tp_transfer.o(i.screen_spim_io_init) refers to hal_gpio.o(i.hal_gpio_config_pad) for hal_gpio_config_pad
    app_tp_transfer.o(i.screen_spim_io_init) refers to app_tp_transfer.o(.constdata) for .constdata
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to app_tp_for_custom_s8.o(.data) for start_now
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to app_tp_for_custom_s8.o(.constdata) for phone_60_start_back
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to app_tp_transfer.o(i.app_tp_screen_init) for app_tp_screen_init
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to app_tp_for_custom_s8.o(.data) for app_tp_count
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to ffltui.o(.text) for __aeabi_ui2f
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to fmul.o(.text) for __aeabi_fmul
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to fdiv.o(.text) for __aeabi_fdiv
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to ffixui.o(.text) for __aeabi_f2uiz
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to f2d.o(.text) for __aeabi_f2d
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to dmul.o(.text) for __aeabi_dmul
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to ddiv.o(.text) for __aeabi_ddiv
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to dfixui.o(.text) for __aeabi_d2uiz
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to app_tp_for_custom_s8.o(.data) for phone_reg_coord_BUF_NUM
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to app_tp_for_custom_s8.o(.bss) for Touch
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_for_custom_s8.o(i.app_tp_write_other_operations) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_for_custom_s8.o(i.app_tp_write_other_operations) refers to app_tp_for_custom_s8.o(.data) for start_now
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.constdata) for screen_87_data
    s8_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) for hal_dsi_rx_ctrl_send_ack_cmd
    s8_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) for hal_dsi_rx_ctrl_get_max_ret_size
    s8_demo.o(i.ap_dcs_read) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.ap_dcs_read) refers to s8_demo.o(.data) for g_rx_ctrl_handle
    s8_demo.o(i.ap_dcs_set_backlight) refers to idiv.o(.text) for __aeabi_idivmod
    s8_demo.o(i.ap_dcs_set_backlight) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    s8_demo.o(i.ap_dcs_set_backlight) refers to s8_demo.o(.data) for AP_REG51_7FF
    s8_demo.o(i.ap_dcs_set_display_off) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.ap_dcs_set_display_off) refers to s8_demo.o(.data) for panel_display_done
    s8_demo.o(i.ap_dcs_set_display_on) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    s8_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to tau_delay.o(i.delayMs) for delayMs
    s8_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    s8_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to s8_demo.o(.data) for sg_system_suspend
    s8_demo.o(i.ap_dcs_set_exit_sleep_mode) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    s8_demo.o(i.ap_dcs_set_exit_sleep_mode) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.ap_dcs_set_exit_sleep_mode) refers to s8_demo.o(.data) for panel_display_done
    s8_demo.o(i.ap_dcs_set_eye_protection_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) for hal_dsi_tx_ctrl_set_ccm
    s8_demo.o(i.ap_rstn_pull_down_cb) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    s8_demo.o(i.ap_rstn_pull_down_cb) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.ap_rstn_pull_down_cb) refers to s8_demo.o(.data) for sg_system_suspend
    s8_demo.o(i.ap_rstn_pull_high_cb) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    s8_demo.o(i.ap_rstn_pull_high_cb) refers to s8_demo.o(.data) for sg_system_resume
    s8_demo.o(i.ap_set_framerate) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.ap_set_framerate) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode) for hal_dsi_tx_ctrl_set_tear_mode
    s8_demo.o(i.ap_set_framerate) refers to s8_demo.o(.data) for g_tx_ctrl_handle
    s8_demo.o(i.ap_update_pps_9E) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) for hal_dsi_rx_ctrl_pre_init_pps
    s8_demo.o(i.ap_update_pps_9E) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) for hal_dsi_rx_ctrl_toggle_resolution
    s8_demo.o(i.ap_update_pps_9E) refers to s8_demo.o(.data) for g_rx_ctrl_handle
    s8_demo.o(i.app_display_init) refers to s8_demo.o(i.app_mipi_rx_init) for app_mipi_rx_init
    s8_demo.o(i.app_display_init) refers to hal_pwr.o(i.hal_pwr_get_vcc_power_ready) for hal_pwr_get_vcc_power_ready
    s8_demo.o(i.app_display_init) refers to s8_demo.o(i.app_gpio_init) for app_gpio_init
    s8_demo.o(i.app_display_init) refers to hal_swire.o(i.hal_swire_init) for hal_swire_init
    s8_demo.o(i.app_display_init) refers to hal_swire.o(i.hal_swire_set_timer) for hal_swire_set_timer
    s8_demo.o(i.app_display_init) refers to s8_demo.o(i.app_mipi_tx_init) for app_mipi_tx_init
    s8_demo.o(i.app_display_init) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.app_gpio_init) refers to memcpya.o(.text) for __aeabi_memcpy4
    s8_demo.o(i.app_gpio_init) refers to hal_gpio.o(i.hal_gpio_config_pad) for hal_gpio_config_pad
    s8_demo.o(i.app_gpio_init) refers to s8_demo.o(.constdata) for .constdata
    s8_demo.o(i.app_init_panel) refers to s8_demo.o(i.app_tx_panel_reset) for app_tx_panel_reset
    s8_demo.o(i.app_init_panel) refers to s8_demo.o(i.send_panel_init_code) for send_panel_init_code
    s8_demo.o(i.app_init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    s8_demo.o(i.app_init_panel) refers to tau_delay.o(i.delayMs) for delayMs
    s8_demo.o(i.app_init_panel) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    s8_demo.o(i.app_init_panel) refers to s8_demo.o(i.soft_swire_init) for soft_swire_init
    s8_demo.o(i.app_init_panel) refers to hal_swire.o(i.hal_swire_enable) for hal_swire_enable
    s8_demo.o(i.app_init_panel) refers to hal_swire.o(i.hal_swire_set_pulse) for hal_swire_set_pulse
    s8_demo.o(i.app_init_panel) refers to s8_demo.o(.constdata) for panel_init_code
    s8_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) for hal_dsi_rx_ctrl_create_handle
    s8_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) for hal_dsi_rx_ctrl_pre_init_pps
    s8_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    s8_demo.o(i.app_mipi_rx_init) refers to s8_demo.o(i.app_set_dcs_hw_ack) for app_set_dcs_hw_ack
    s8_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    s8_demo.o(i.app_mipi_rx_init) refers to s8_demo.o(.data) for g_rx_ctrl_handle
    s8_demo.o(i.app_mipi_rx_init) refers to s8_demo.o(.constdata) for g_cus_rx_dcs_execute_table
    s8_demo.o(i.app_mipi_rx_init) refers to s8_demo.o(i.pps_update_handle) for pps_update_handle
    s8_demo.o(i.app_mipi_rx_start_cb) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    s8_demo.o(i.app_mipi_rx_start_cb) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    s8_demo.o(i.app_mipi_rx_start_cb) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.app_mipi_rx_start_cb) refers to s8_demo.o(.data) for g_rx_ctrl_handle
    s8_demo.o(i.app_mipi_tx_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) for hal_dsi_tx_ctrl_create_handle
    s8_demo.o(i.app_mipi_tx_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    s8_demo.o(i.app_mipi_tx_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) for hal_dsi_tx_ctrl_set_overwrite_rgb
    s8_demo.o(i.app_mipi_tx_init) refers to s8_demo.o(.data) for g_tx_ctrl_handle
    s8_demo.o(i.app_mipi_tx_start) refers to s8_demo.o(i.app_init_panel) for app_init_panel
    s8_demo.o(i.app_mipi_tx_start) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    s8_demo.o(i.app_mipi_tx_start) refers to tau_delay.o(i.delayMs) for delayMs
    s8_demo.o(i.app_mipi_tx_start) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    s8_demo.o(i.app_mipi_tx_start) refers to hal_swire.o(i.hal_swire_set_pulse) for hal_swire_set_pulse
    s8_demo.o(i.app_mipi_tx_start) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.app_mipi_tx_start) refers to s8_demo.o(.data) for g_tx_ctrl_handle
    s8_demo.o(i.app_set_dcs_hw_ack) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack) for hal_dsi_rx_ctrl_set_auto_ack
    s8_demo.o(i.app_set_dcs_hw_ack) refers to s8_demo.o(.data) for g_rx_ctrl_handle
    s8_demo.o(i.app_system_process) refers to s8_demo.o(i.app_system_suspend) for app_system_suspend
    s8_demo.o(i.app_system_process) refers to s8_demo.o(i.app_system_resume) for app_system_resume
    s8_demo.o(i.app_system_process) refers to s8_demo.o(i.app_mipi_tx_start) for app_mipi_tx_start
    s8_demo.o(i.app_system_process) refers to s8_demo.o(.data) for sg_system_suspend
    s8_demo.o(i.app_system_resume) refers to hal_pwr.o(i.hal_pwr_exit_sleep_mode) for hal_pwr_exit_sleep_mode
    s8_demo.o(i.app_system_resume) refers to s8_demo.o(i.app_display_init) for app_display_init
    s8_demo.o(i.app_system_resume) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.app_system_suspend) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) for hal_dsi_tx_ctrl_stop
    s8_demo.o(i.app_system_suspend) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) for hal_dsi_tx_ctrl_deinit
    s8_demo.o(i.app_system_suspend) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) for hal_dsi_rx_ctrl_stop
    s8_demo.o(i.app_system_suspend) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) for hal_dsi_rx_ctrl_deinit
    s8_demo.o(i.app_system_suspend) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    s8_demo.o(i.app_system_suspend) refers to hal_swire.o(i.hal_swire_deinit) for hal_swire_deinit
    s8_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_set_sleep_mode_power) for hal_pwr_set_sleep_mode_power
    s8_demo.o(i.app_system_suspend) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    s8_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_enter_normal_sleep_mode) for hal_pwr_enter_normal_sleep_mode
    s8_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) for hal_pwr_set_stop_sleep_wakeup_pin
    s8_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) for hal_pwr_enter_stop_sleep_mode
    s8_demo.o(i.app_system_suspend) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode) for hal_pwr_enter_deep_sleep_mode
    s8_demo.o(i.app_system_suspend) refers to s8_demo.o(.data) for g_tx_ctrl_handle
    s8_demo.o(i.app_system_suspend) refers to s8_demo.o(i.ap_rstn_pull_high_cb) for ap_rstn_pull_high_cb
    s8_demo.o(i.app_tx_panel_reset) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    s8_demo.o(i.app_tx_panel_reset) refers to tau_delay.o(i.delayMs) for delayMs
    s8_demo.o(i.pps_update_handle) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) for hal_dsi_rx_ctrl_toggle_resolution
    s8_demo.o(i.pps_update_handle) refers to s8_demo.o(.data) for g_rx_ctrl_handle
    s8_demo.o(i.s8_demo) refers to hal_pwr.o(i.hal_pwr_set_main_power) for hal_pwr_set_main_power
    s8_demo.o(i.s8_demo) refers to s8_demo.o(i.app_display_init) for app_display_init
    s8_demo.o(i.s8_demo) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.s8_demo) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) for hal_dsi_rx_ctrl_dcs_async_handler
    s8_demo.o(i.s8_demo) refers to s8_demo.o(i.app_system_process) for app_system_process
    s8_demo.o(i.s8_demo) refers to s8_demo.o(.data) for g_rx_ctrl_handle
    s8_demo.o(i.send_panel_init_code) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) for hal_dsi_tx_ctrl_write_array_cmd
    s8_demo.o(i.send_panel_init_code) refers to tau_delay.o(i.delayUs) for delayUs
    s8_demo.o(i.soft_swire_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    s8_demo.o(i.soft_swire_init) refers to tau_delay.o(i.delayMs) for delayMs
    s8_demo.o(i.soft_swire_init) refers to s8_demo.o(i.soft_swire_start) for soft_swire_start
    s8_demo.o(i.soft_swire_init) refers to hal_timer.o(i.hal_timer_init) for hal_timer_init
    s8_demo.o(i.soft_swire_init) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    s8_demo.o(i.soft_swire_init) refers to s8_demo.o(.data) for s_swire_pwm_counter
    s8_demo.o(i.soft_swire_init) refers to s8_demo.o(i.soft_swire_timer_callback) for soft_swire_timer_callback
    s8_demo.o(i.soft_swire_start) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    s8_demo.o(i.soft_swire_start) refers to tau_delay.o(i.delayUs) for delayUs
    s8_demo.o(i.soft_swire_timer_callback) refers to s8_demo.o(i.soft_swire_start) for soft_swire_start
    s8_demo.o(i.soft_swire_timer_callback) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    s8_demo.o(i.soft_swire_timer_callback) refers to hal_timer.o(i.hal_timer_deinit) for hal_timer_deinit
    s8_demo.o(i.soft_swire_timer_callback) refers to hal_timer.o(i.hal_timer_stop) for hal_timer_stop
    s8_demo.o(i.soft_swire_timer_callback) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    s8_demo.o(i.soft_swire_timer_callback) refers to s8_demo.o(.data) for s_swire_pwm_counter
    s8_demo.o(.constdata) refers to s8_demo.o(i.ap_dcs_set_display_on) for ap_dcs_set_display_on
    s8_demo.o(.constdata) refers to s8_demo.o(i.ap_dcs_set_display_off) for ap_dcs_set_display_off
    s8_demo.o(.constdata) refers to s8_demo.o(i.ap_dcs_set_backlight) for ap_dcs_set_backlight
    s8_demo.o(.constdata) refers to s8_demo.o(i.ap_dcs_set_enter_sleep_mode) for ap_dcs_set_enter_sleep_mode
    s8_demo.o(.constdata) refers to s8_demo.o(i.ap_dcs_set_exit_sleep_mode) for ap_dcs_set_exit_sleep_mode
    s8_demo.o(.constdata) refers to s8_demo.o(i.ap_update_pps_9E) for ap_update_pps_9E
    s8_demo.o(.constdata) refers to s8_demo.o(i.ap_set_framerate) for ap_set_framerate
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_init) for hal_system_init
    board.o(i.board_Init) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    board.o(i.board_Init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    board.o(i.board_Init) refers to tau_log.o(i.tau_log_init) for tau_log_init
    startup_armcm0.o(RESET) refers to startup_armcm0.o(STACK) for __initial_sp
    startup_armcm0.o(RESET) refers to startup_armcm0.o(.text) for Reset_Handler
    startup_armcm0.o(RESET) refers to drv_common.o(i.HardFault_Handler) for HardFault_Handler
    startup_armcm0.o(RESET) refers to drv_common.o(i.SysTick_Handler) for SysTick_Handler
    startup_armcm0.o(RESET) refers to drv_vidc.o(i.VIDC_IRQn_Handler) for VIDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to hal_internal_vsync.o(i.LCDC_IRQn_Handler) for LCDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) for MIPI_RX_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler) for MIPI_TX_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_memc.o(i.MEMC_IRQn_Handler) for MEMC_IRQn_Handler
    startup_armcm0.o(RESET) refers to hal_internal_dcs.o(i.VPRE_IRQn_Handler) for VPRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_dma.o(i.DMA_IRQn_Handler) for DMA_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER0_IRQn_Handler) for TIMER0_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER1_IRQn_Handler) for TIMER1_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER2_IRQn_Handler) for TIMER2_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER3_IRQn_Handler) for TIMER3_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_wdg.o(i.WDG_IRQn_Handler) for WDG_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_uart.o(i.UART_IRQn_Handler) for UART_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_i2c.o(i.I2C0_IRQn_Handler) for I2C0_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_i2c.o(i.I2C1_IRQn_Handler) for I2C1_IRQn_Handler
    startup_armcm0.o(RESET) refers to hal_spi_master.o(i.SPIM_IRQn_Handler) for SPIM_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_rxbr.o(i.VPRE1_IRQn_Handler) for VPRE1_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_i2c.o(i.I2C2_IRQn_Handler) for I2C2_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_swire.o(i.SWIRE_IRQn_Handler) for SWIRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.AP_NRESET_IRQn_Handler) for AP_NRESET_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT0_IRQn_Handler) for EXTI_INT0_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT1_IRQn_Handler) for EXTI_INT1_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT2_IRQn_Handler) for EXTI_INT2_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT3_IRQn_Handler) for EXTI_INT3_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT4_IRQn_Handler) for EXTI_INT4_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT5_IRQn_Handler) for EXTI_INT5_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT6_IRQn_Handler) for EXTI_INT6_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT7_IRQn_Handler) for EXTI_INT7_IRQn_Handler
    startup_armcm0.o(.text) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    demo_hal_crc.o(i.demo_crc_array_dma_cal) refers to hal_crc.o(i.hal_crc_dma_init) for hal_crc_dma_init
    demo_hal_crc.o(i.demo_crc_array_dma_cal) refers to hal_crc.o(i.hal_crc_dma_start) for hal_crc_dma_start
    demo_hal_crc.o(i.demo_crc_array_dma_cal) refers to demo_hal_crc.o(.constdata) for .constdata
    demo_hal_crc.o(i.demo_crc_array_dma_cal) refers to demo_hal_crc.o(.data) for sg_crc32_arry
    demo_hal_crc.o(i.demo_crc_array_dma_cal) refers to demo_hal_crc.o(i.demo_crc_dma_callback) for demo_crc_dma_callback
    demo_hal_crc.o(i.demo_crc_dma_callback) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    demo_hal_crc.o(i.demo_hal_crc_case) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    demo_hal_crc.o(i.demo_hal_crc_case) refers to demo_hal_crc.o(i.demo_crc_array_dma_cal) for demo_crc_array_dma_cal
    demo_hal_dsi_rx.o(i.ap_dcs_read) refers to memcpya.o(.text) for __aeabi_memcpy4
    demo_hal_dsi_rx.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd) for hal_dsi_rx_ctrl_ack_long_cmd
    demo_hal_dsi_rx.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) for hal_dsi_rx_ctrl_get_max_ret_size
    demo_hal_dsi_rx.o(i.ap_dcs_read) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    demo_hal_dsi_rx.o(i.ap_dcs_read) refers to demo_hal_dsi_rx.o(.constdata) for .constdata
    demo_hal_dsi_rx.o(i.ap_dcs_read) refers to demo_hal_dsi_rx.o(.data) for g_rx_ctrl_handle
    demo_hal_dsi_rx.o(i.cus_dsc_execute) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    demo_hal_dsi_rx.o(i.cus_dsc_execute) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) for hal_dsi_rx_ctrl_send_ack_cmd
    demo_hal_dsi_rx.o(i.cus_dsc_execute) refers to demo_hal_dsi_rx.o(.data) for g_rx_ctrl_handle
    demo_hal_dsi_rx.o(i.demo_hal_dsi_rx_case) refers to demo_hal_dsi_rx.o(i.open_mipi_rx) for open_mipi_rx
    demo_hal_dsi_rx.o(i.demo_hal_dsi_rx_case) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    demo_hal_dsi_rx.o(i.demo_hal_dsi_rx_case) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) for hal_dsi_rx_ctrl_dcs_async_handler
    demo_hal_dsi_rx.o(i.demo_hal_dsi_rx_case) refers to demo_hal_dsi_rx.o(.data) for g_rx_ctrl_handle
    demo_hal_dsi_rx.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) for hal_dsi_rx_ctrl_create_handle
    demo_hal_dsi_rx.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    demo_hal_dsi_rx.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    demo_hal_dsi_rx.o(i.open_mipi_rx) refers to demo_hal_dsi_rx.o(.data) for g_rx_ctrl_handle
    demo_hal_dsi_rx.o(i.open_mipi_rx) refers to demo_hal_dsi_rx.o(.constdata) for g_cus_rx_dcs_execute_table
    demo_hal_dsi_rx.o(i.open_mipi_rx) refers to demo_hal_dsi_rx.o(i.ap_dcs_read) for ap_dcs_read
    demo_hal_dsi_rx.o(.constdata) refers to demo_hal_dsi_rx.o(i.cus_dsc_execute) for cus_dsc_execute
    demo_hal_dsi_tx.o(i.demo_dsi_tx_case) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    demo_hal_dsi_tx.o(i.demo_dsi_tx_case) refers to demo_hal_dsi_tx.o(i.demo_open_mipi_rx) for demo_open_mipi_rx
    demo_hal_dsi_tx.o(i.demo_dsi_tx_case) refers to demo_hal_dsi_tx.o(i.demo_open_mipi_tx) for demo_open_mipi_tx
    demo_hal_dsi_tx.o(i.demo_open_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) for hal_dsi_tx_ctrl_create_handle
    demo_hal_dsi_tx.o(i.demo_open_mipi_tx) refers to memcpya.o(.text) for __aeabi_memcpy4
    demo_hal_dsi_tx.o(i.demo_open_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    demo_hal_dsi_tx.o(i.demo_open_mipi_tx) refers to demo_hal_dsi_tx.o(i.demo_panel_init) for demo_panel_init
    demo_hal_dsi_tx.o(i.demo_open_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    demo_hal_dsi_tx.o(i.demo_open_mipi_tx) refers to demo_hal_dsi_tx.o(.data) for g_tx_ctrl_handle
    demo_hal_dsi_tx.o(i.demo_panel_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    demo_hal_dsi_tx.o(i.demo_panel_init) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    demo_hal_dsi_tx.o(i.demo_panel_init) refers to tau_delay.o(i.delayMs) for delayMs
    demo_hal_dsi_tx.o(i.demo_panel_init) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    demo_hal_dsi_tx.o(i.demo_panel_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    demo_hal_wdg.o(i.demo_wdg_callback) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    demo_hal_wdg.o(i.demo_wdg_callback) refers to hal_wdg.o(i.hal_wdg_stop) for hal_wdg_stop
    demo_hal_wdg.o(i.demo_wdg_callback) refers to demo_hal_wdg.o(.data) for sg_wdg_io_lvl
    demo_hal_wdg.o(i.demo_wdg_case) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    demo_hal_wdg.o(i.demo_wdg_case) refers to demo_hal_wdg.o(i.demo_wdg_case_int_mode) for demo_wdg_case_int_mode
    demo_hal_wdg.o(i.demo_wdg_case_int_mode) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    demo_hal_wdg.o(i.demo_wdg_case_int_mode) refers to hal_wdg.o(i.hal_wdg_init) for hal_wdg_init
    demo_hal_wdg.o(i.demo_wdg_case_int_mode) refers to hal_wdg.o(i.hal_wdg_set_repeat) for hal_wdg_set_repeat
    demo_hal_wdg.o(i.demo_wdg_case_int_mode) refers to hal_wdg.o(i.hal_wdg_register_callback) for hal_wdg_register_callback
    demo_hal_wdg.o(i.demo_wdg_case_int_mode) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    demo_hal_wdg.o(i.demo_wdg_case_int_mode) refers to hal_wdg.o(i.hal_wdg_start) for hal_wdg_start
    demo_hal_wdg.o(i.demo_wdg_case_int_mode) refers to hal_wdg.o(i.hal_wdg_kick_dog) for hal_wdg_kick_dog
    demo_hal_wdg.o(i.demo_wdg_case_int_mode) refers to tau_delay.o(i.delayMs) for delayMs
    demo_hal_wdg.o(i.demo_wdg_case_int_mode) refers to demo_hal_wdg.o(i.demo_wdg_callback) for demo_wdg_callback
    demo_hal_wdg.o(i.demo_wdg_case_int_mode) refers to demo_hal_wdg.o(.data) for sg_wdg_io_lvl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd) refers to drv_rxbr.o(i.drv_rxbr_set_ack_pkt_md) for drv_rxbr_set_ack_pkt_md
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_lpdt_fifo_status) for drv_dsi_rx_get_lpdt_fifo_status
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) for dcs_packet_get_fifo_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) for dcs_packet_free_fifo_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) for hal_internal_vsync_get_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_reset_modules) for drv_crgu_reset_modules
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_rxbr.o(i.drv_rxbr_swpxl_clr) for drv_rxbr_swpxl_clr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_rxbr.o(i.drv_rxbr_set_swpxl_data) for drv_rxbr_set_swpxl_data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg) for drv_dsi_rx_set_ddi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) for hal_dsi_rx_ctrl_set_rx_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg) for drv_dsi_rx_set_ipi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.constdata) for .constdata
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_force_video_crtl) refers to drv_dsi_rx.o(i.drv_dsi_rx_force_video_crtl) for drv_dsi_rx_force_video_crtl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size) for drv_dsi_rx_get_max_ret_size
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) for hal_dsi_rx_ctrl_init_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_rx) for hal_internal_vsync_init_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) for hal_dsi_rx_ctrl_init_dsi_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) for hal_dsi_rx_ctrl_init_rxbr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) for hal_dsi_rx_ctrl_init_vidc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) for hal_dsi_rx_ctrl_init_memc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_se.o(i.drv_se_start_rx) for drv_se_start_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_pwr.o(i.drv_pwr_set_pll_clk) for drv_pwr_set_pll_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_clk) for drv_crgu_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dsc_clk) for drv_crgu_set_dsc_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_vidc_clk) for drv_crgu_set_vidc_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_fb_clk) for drv_crgu_set_fb_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg) for drv_dsi_rx_set_ctrl_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) for drv_dsi_rx_set_up_phy
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap) for drv_dsi_rx_set_lane_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_crc_en) for drv_dsi_rx_set_ddi_crc_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_ycbcr_frmt) for drv_dsi_rx_set_ipi_ycbcr_frmt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_tear_resp_en) for drv_dsi_rx_set_tear_resp_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_inten) for drv_dsi_rx_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc) for drv_dsi_rx_set_check_crc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt) for drv_dsi_rx_set_resp_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_mode) for drv_memc_set_ltpo_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_fs_en_conditions) for drv_memc_set_fs_en_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_lcdc_st_conditions) for drv_memc_set_lcdc_st_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_vidc_sync_cnt) for drv_memc_set_vidc_sync_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_double_buffer) for drv_memc_set_double_buffer
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_circ_mode_enable) for drv_memc_set_circ_mode_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_active_height) for drv_memc_set_active_height
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_pu_thres) for drv_memc_set_ltpo_pu_thres
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_color_format) for drv_rxbr_set_color_format
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th) for drv_rxbr_set_ltpo_drop_th
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_cfg) for drv_rxbr_set_usr_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_col) for drv_rxbr_set_usr_col
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_row) for drv_rxbr_set_usr_row
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg) for drv_rxbr_hline_rcv_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) for hal_intl_dcs_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_src_parameter) for drv_vidc_set_src_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pentile_swap) for drv_vidc_set_pentile_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_dst_parameter) for drv_vidc_set_dst_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_circ_mode_enable) for drv_vidc_set_circ_mode_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_init_module_enable) for drv_vidc_init_module_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_dither_config) for drv_vidc_set_dither_config
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_vintp_config) for drv_vidc_set_vintp_config
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_rotation) for drv_vidc_set_rotation
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef0) for drv_vidc_set_scld_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef1) for drv_vidc_set_scld_hcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef0) for drv_vidc_set_scld_vcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef1) for drv_vidc_set_scld_vcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_honly_hinitr) for drv_vidc_set_honly_hinitr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_honly_hinitb) for drv_vidc_set_honly_hinitb
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_honly_hcoef0) for drv_vidc_set_honly_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_mirror) for drv_vidc_set_mirror
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pu_ctrl) for drv_vidc_set_pu_ctrl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_dsi_rx_ctrl.o(.constdata) for .constdata
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to hal_internal_vsync.o(i.hal_internal_sync_register_rx_callback) for hal_internal_sync_register_rx_callback
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to drv_vidc.o(i.drv_vidc_set_irq_line) for drv_vidc_set_irq_line
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_write_cmd_entry) refers to hal_internal_dcs.o(i.hal_intl_dcs_register_write_cmd_entry) for hal_intl_dcs_register_write_cmd_entry
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header) for drv_rxbr_set_ack_pkt_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack) refers to drv_rxbr.o(i.drv_rxbr_set_cmd_response) for drv_rxbr_set_cmd_response
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) for hal_intl_dcs_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_check_crc) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc) for drv_dsi_rx_set_check_crc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_check_crc) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) for drv_dsi_rx_calc_ipi_tx_delay
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg) for drv_dsi_rx_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_log_level) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_drv_log_level) for drv_dsi_rx_set_drv_log_level
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to drv_rxbr.o(i.drv_rxbr_clr_swp_cnt) for drv_rxbr_clr_swp_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to drv_rxbr.o(i.drv_rxbr_set_col_addr) for drv_rxbr_set_col_addr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to drv_rxbr.o(i.drv_rxbr_set_page_addr) for drv_rxbr_set_page_addr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to drv_rxbr.o(i.drv_rxbr_set_swpxl_data) for drv_rxbr_set_swpxl_data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) for hal_dsi_rx_ctrl_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) for hal_intl_svs_update_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_clk) for drv_crgu_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_dsi_rx.o(i.drv_dsi_rx_power_up) for drv_dsi_rx_power_up
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) for hal_internal_vsync_toggle_input_frame_rate
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) for hal_internal_sync_input_resolution_change
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) for hal_dsi_tx_ctrl_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg) for drv_dsi_tx_phy_time_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) for drv_dsi_tx_phy_test_setup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready) for drv_dsi_tx_phy_status_ready
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_crgu.o(i.drv_crgu_reset_modules) for drv_crgu_reset_modules
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_reset_modules) for drv_crgu_reset_modules
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb) for hal_internal_sync_register_lcdc_cb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_frame) refers to drv_lcdc.o(i.drv_lcdc_fixed_frame_output) for drv_lcdc_fixed_frame_output
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_get_tear_mode) for drv_memc_get_tear_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_gen_a_tear_signal) for drv_memc_gen_a_tear_signal
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_tx) for hal_internal_vsync_init_tx
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb) for hal_internal_sync_register_lcdc_cb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) for hal_dsi_tx_ctrl_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) for hal_dsi_tx_init_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) for hal_dsi_tx_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) for hal_lcdc_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) for hal_lcdc_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready) for drv_dsi_tx_phy_status_ready
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_func_update) for hal_lcdc_func_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_overwrite_enable) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_overwrite_enable) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload) for drv_dsi_tx_command_get_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_sync_line) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) for hal_internal_vsync_set_sync_line
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_sync_line) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb) for drv_lcdc_config_overwrite_rgb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_vpg) for drv_dsi_tx_set_vpg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_cfg_int_frame) for drv_lcdc_cfg_int_frame
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_enable_shadow_reg) for drv_lcdc_enable_shadow_reg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_start) for hal_lcdc_start
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_lcdc.o(i.drv_lcdc_stop_display) for drv_lcdc_stop_display
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) for hal_dsi_tx_ctrl_read_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg) for drv_dsi_tx_video_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack) for drv_dsi_tx_set_bta_ack
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time) for drv_dsi_tx_dpi_lpcmd_time
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode) for drv_dsi_tx_phy_lane_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode) for drv_dsi_tx_dpi_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity) for drv_dsi_tx_dpi_polarity
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_response_mode) for drv_dsi_tx_response_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div) for drv_dsi_tx_set_time_out_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg) for drv_dsi_tx_timeout_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp) for drv_dsi_tx_phy_clock_lane_auto_lp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_int) for drv_dsi_tx_config_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to drv_crgu.o(i.drv_crgu_set_dpi_clk) for drv_crgu_set_dpi_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to hal_dsi_tx_ctrl.o(.constdata) for .constdata
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg) for drv_dsi_tx_phy_time_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) for drv_dsi_tx_phy_test_setup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update) for hal_dsi_tx_timing_info_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) for hal_dsi_tx_cmd_mode_cal_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size) for drv_dsi_tx_edpi_cmd_size
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) for hal_dsi_tx_init_phy_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) for hal_dsi_tx_init_dpi_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) for hal_dsi_tx_vid_mode_cal_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing) for hal_dsi_tx_init_vid_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk) for drv_dsi_tx_set_video_chunk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing) for drv_dsi_tx_set_video_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_header) for drv_dsi_tx_command_header
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update) refers to d2f.o(.text) for __aeabi_d2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_internal_svs.o(i.hal_intl_svs_init_tx) for hal_intl_svs_init_tx
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) for hal_tx_frame_rate_adjust
    hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) refers to drv_lcdc.o(i.drv_lcdc_endianness_config) for drv_lcdc_endianness_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) refers to drv_lcdc.o(i.drv_lcdc_crop_hact) for drv_lcdc_crop_hact
    hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_lcdc_func_update) refers to drv_lcdc.o(i.drv_lcdc_bcsa_config) for drv_lcdc_bcsa_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_func_update) refers to drv_lcdc.o(i.drv_lcdc_fc_config) for drv_lcdc_fc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_func_update) refers to drv_lcdc.o(i.drv_lcdc_edge_dect_config) for drv_lcdc_edge_dect_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_func_update) refers to drv_lcdc.o(i.drv_lcdc_edge_enh_config) for drv_lcdc_edge_enh_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_func_update) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_lcdc_func_update) refers to hal_dsi_tx_ctrl.o(.data) for sg_vsync_flag
    hal_dsi_tx_ctrl.o(i.hal_lcdc_func_update) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for sg_pq_para
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) for hal_lcdc_postproc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) for hal_lcdc_displayproc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) for hal_intl_fb_get_tx_fb_info
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) for hal_lcdc_timinggen_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to drv_lcdc.o(i.drv_lcdc_config_int) for drv_lcdc_config_int
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fscalb.o(.text) for __ARM_scalbnf
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_lcdc_clk) for drv_crgu_set_lcdc_clk
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) for hal_intl_fb_get_tx_fb_info
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) for hal_lcdc_upscaler_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_fldc_config) for drv_lcdc_fldc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_bcsa_config) for drv_lcdc_bcsa_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_fc_config) for drv_lcdc_fc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_edge_dect_config) for drv_lcdc_edge_dect_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_edge_enh_config) for drv_lcdc_edge_enh_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_vintp_mode_config) for drv_lcdc_vintp_mode_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_dith_config) for drv_lcdc_dith_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to drv_lcdc.o(i.drv_lcdc_vid_hw_start) for drv_lcdc_vid_hw_start
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to drv_lcdc.o(i.drv_lcdc_cmd_start) for drv_lcdc_cmd_start
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to drv_lcdc.o(i.drv_lcdc_ctrl_flow) for drv_lcdc_ctrl_flow
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to drv_lcdc.o(i.drv_lcdc_config_src_parameter) for drv_lcdc_config_src_parameter
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to drv_lcdc.o(i.drv_lcdc_set_prefetch) for drv_lcdc_set_prefetch
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to cfcmple.o(.text) for __aeabi_cfcmple
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_gpio.o(i.hal_gpio_config_pad) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_config_pad) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    hal_gpio.o(i.hal_gpio_config_pad) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    hal_gpio.o(i.hal_gpio_ctrl_eint) refers to drv_gpio.o(i.drv_gpio_set_int) for drv_gpio_set_int
    hal_gpio.o(i.hal_gpio_ctrl_eint) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_get_input_data) refers to drv_gpio.o(i.drv_gpio_get_input_data) for drv_gpio_get_input_data
    hal_gpio.o(i.hal_gpio_get_int_type) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_eint) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group) for drv_sys_cfg_sel_gpio_group
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig) for drv_sys_cfg_sel_int_trig
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_init_eint) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_input) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_input) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_input) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_init_output) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_reg_eint_cb) refers to drv_gpio.o(i.drv_gpio_register_callback) for drv_gpio_register_callback
    hal_gpio.o(i.hal_gpio_reg_eint_cb) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_gpio.o(i.drv_gpio_register_ap_reset_callback) for drv_gpio_register_ap_reset_callback
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) for drv_sys_cfg_sel_ap_rst_trig
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_high_impedance) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_gpio.o(i.hal_gpio_set_high_impedance) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode) for drv_gpio_set_mode
    hal_gpio.o(i.hal_gpio_set_mode) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_output_data) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to hal_gpio.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_i2c.o(i.drv_i2c_get_intr_status) for drv_i2c_get_intr_status
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_i2c.o(i.drv_i2c_get_rx_count) for drv_i2c_get_rx_count
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_i2c.o(i.drv_i2c_flush) for drv_i2c_flush
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_i2c.o(i.drv_i2c_clear_intr_status) for drv_i2c_clear_intr_status
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_dma.o(i.drv_dma_enable) for drv_dma_enable
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_deinit) refers to drv_dma.o(i.drv_dma_deinit) for drv_dma_deinit
    hal_i2c_slave.o(i.hal_i2cs_deinit) refers to drv_i2c.o(i.drv_i2c_clock_enable) for drv_i2c_clock_enable
    hal_i2c_slave.o(i.hal_i2cs_deinit) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_get_rx_cnt) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_get_tx_cnt) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_get_write_complete) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_init) refers to drv_i2c.o(i.drv_i2c_clock_enable) for drv_i2c_clock_enable
    hal_i2c_slave.o(i.hal_i2cs_init) refers to drv_i2c.o(i.drv_i2cs_init) for drv_i2cs_init
    hal_i2c_slave.o(i.hal_i2cs_init) refers to drv_i2c.o(i.drv_i2c_set_callback) for drv_i2c_set_callback
    hal_i2c_slave.o(i.hal_i2cs_init) refers to drv_dma.o(i.drv_dma_apply_handle) for drv_dma_apply_handle
    hal_i2c_slave.o(i.hal_i2cs_init) refers to drv_dma.o(i.drv_dma_set_bitwide) for drv_dma_set_bitwide
    hal_i2c_slave.o(i.hal_i2cs_init) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    hal_i2c_slave.o(i.hal_i2cs_init) refers to hal_i2c_slave.o(i.hal_i2cs_callback) for hal_i2cs_callback
    hal_i2c_slave.o(i.hal_i2cs_init) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_register_callback) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_rx_cnt_clear) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_start) refers to drv_i2c.o(i.drv_i2c_enable_intr) for drv_i2c_enable_intr
    hal_i2c_slave.o(i.hal_i2cs_start) refers to drv_i2c.o(i.drv_i2c_enable) for drv_i2c_enable
    hal_i2c_slave.o(i.hal_i2cs_start) refers to drv_i2c.o(i.drv_i2c_enable_dma_req) for drv_i2c_enable_dma_req
    hal_i2c_slave.o(i.hal_i2cs_start) refers to drv_dma.o(i.drv_dma_register_callback) for drv_dma_register_callback
    hal_i2c_slave.o(i.hal_i2cs_start) refers to drv_dma.o(i.drv_dma_enable_int) for drv_dma_enable_int
    hal_i2c_slave.o(i.hal_i2cs_start) refers to drv_dma.o(i.drv_dma_enable) for drv_dma_enable
    hal_i2c_slave.o(i.hal_i2cs_start) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_start) refers to hal_i2c_slave.o(i.hal_i2cs_tx_dma_callback) for hal_i2cs_tx_dma_callback
    hal_i2c_slave.o(i.hal_i2cs_stop) refers to drv_i2c.o(i.drv_i2c_enable) for drv_i2c_enable
    hal_i2c_slave.o(i.hal_i2cs_stop) refers to drv_i2c.o(i.drv_i2c_disable_intr) for drv_i2c_disable_intr
    hal_i2c_slave.o(i.hal_i2cs_stop) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_i2c_slave.o(i.hal_i2cs_stop) refers to drv_i2c.o(i.drv_i2c_disable_dma_req) for drv_i2c_disable_dma_req
    hal_i2c_slave.o(i.hal_i2cs_stop) refers to drv_i2c.o(i.drv_i2c_flush) for drv_i2c_flush
    hal_i2c_slave.o(i.hal_i2cs_stop) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_tx_dma_callback) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) refers to drv_i2c.o(i.drv_i2c_flush) for drv_i2c_flush
    hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) refers to drv_dma.o(i.drv_dma_set_mem_trans_info) for drv_dma_set_mem_trans_info
    hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) refers to drv_dma.o(i.drv_dma_enable) for drv_dma_enable
    hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer) refers to drv_i2c.o(i.drv_i2c_flush) for drv_i2c_flush
    hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer) refers to drv_dma.o(i.drv_dma_set_mem_trans_info) for drv_dma_set_mem_trans_info
    hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer) refers to drv_dma.o(i.drv_dma_set_circle_mode) for drv_dma_set_circle_mode
    hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer) refers to hal_i2c_slave.o(.data) for .data
    hal_spi_master.o(i.SPIM_IRQn_Handler) refers to drv_spi_master.o(i.drv_spim_get_int_status) for drv_spim_get_int_status
    hal_spi_master.o(i.SPIM_IRQn_Handler) refers to drv_spi_master.o(i.drv_spim_get_busy) for drv_spim_get_busy
    hal_spi_master.o(i.SPIM_IRQn_Handler) refers to drv_spi_master.o(i.drv_spim_disable_int) for drv_spim_disable_int
    hal_spi_master.o(i.SPIM_IRQn_Handler) refers to drv_spi_master.o(i.drv_spim_set_inten) for drv_spim_set_inten
    hal_spi_master.o(i.SPIM_IRQn_Handler) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    hal_spi_master.o(i.SPIM_IRQn_Handler) refers to drv_spi_master.o(i.drv_spim_clear_int_status) for drv_spim_clear_int_status
    hal_spi_master.o(i.SPIM_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_spi_master.o(i.SPIM_IRQn_Handler) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spim_deinit) refers to drv_spi_master.o(i.drv_spim_disable) for drv_spim_disable
    hal_spi_master.o(i.hal_spim_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_spi_master.o(i.hal_spim_flush) refers to drv_spi_master.o(i.drv_spim_flush) for drv_spim_flush
    hal_spi_master.o(i.hal_spim_get_transfer_complete) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spim_init) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_spi_master.o(i.hal_spim_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    hal_spi_master.o(i.hal_spim_init) refers to drv_spi_master.o(i.drv_spim_init) for drv_spim_init
    hal_spi_master.o(i.hal_spim_init) refers to drv_spi_master.o(i.drv_spim_enable) for drv_spim_enable
    hal_spi_master.o(i.hal_spim_read) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    hal_spi_master.o(i.hal_spim_read) refers to drv_spi_master.o(i.drv_spim_read) for drv_spim_read
    hal_spi_master.o(i.hal_spim_read) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spim_write) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    hal_spi_master.o(i.hal_spim_write) refers to drv_spi_master.o(i.drv_spim_write) for drv_spim_write
    hal_spi_master.o(i.hal_spim_write) refers to hal_spi_master.o(.data) for .data
    hal_swire.o(i.hal_swire_deinit) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    hal_swire.o(i.hal_swire_deinit) refers to drv_swire.o(i.drv_swire_enable) for drv_swire_enable
    hal_swire.o(i.hal_swire_deinit) refers to drv_swire.o(i.drv_swire_register_callback) for drv_swire_register_callback
    hal_swire.o(i.hal_swire_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_swire.o(i.hal_swire_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_swire.o(i.hal_swire_deinit) refers to hal_timer.o(i.hal_timer_deinit) for hal_timer_deinit
    hal_swire.o(i.hal_swire_deinit) refers to hal_swire.o(.data) for .data
    hal_swire.o(i.hal_swire_enable) refers to drv_swire.o(i.drv_swire_set_power_down) for drv_swire_set_power_down
    hal_swire.o(i.hal_swire_enable) refers to drv_swire.o(i.drv_swire_get_pulse_count) for drv_swire_get_pulse_count
    hal_swire.o(i.hal_swire_enable) refers to drv_swire.o(i.drv_swire_set_trig_mode) for drv_swire_set_trig_mode
    hal_swire.o(i.hal_swire_enable) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_swire.o(i.hal_swire_enable) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    hal_swire.o(i.hal_swire_enable) refers to hal_swire.o(.data) for .data
    hal_swire.o(i.hal_swire_init) refers to drv_crgu.o(i.drv_crgu_set_clock_div) for drv_crgu_set_clock_div
    hal_swire.o(i.hal_swire_init) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_swire.o(i.hal_swire_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_swire.o(i.hal_swire_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_swire.o(i.hal_swire_init) refers to drv_swire.o(i.drv_swire_set_bit_time) for drv_swire_set_bit_time
    hal_swire.o(i.hal_swire_init) refers to drv_swire.o(i.drv_swire_set_power_down) for drv_swire_set_power_down
    hal_swire.o(i.hal_swire_init) refers to drv_swire.o(i.drv_swire_enable) for drv_swire_enable
    hal_swire.o(i.hal_swire_init) refers to drv_common.o(.data) for g_system_clock
    hal_swire.o(i.hal_swire_register_callback) refers to drv_swire.o(i.drv_swire_register_callback) for drv_swire_register_callback
    hal_swire.o(i.hal_swire_register_callback) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    hal_swire.o(i.hal_swire_set_pulse) refers to drv_swire.o(i.drv_swire_set_trig_mode) for drv_swire_set_trig_mode
    hal_swire.o(i.hal_swire_set_pulse) refers to drv_swire.o(i.drv_swire_set_pulse_count) for drv_swire_set_pulse_count
    hal_swire.o(i.hal_swire_set_pulse) refers to hal_swire.o(.data) for .data
    hal_swire.o(i.hal_swire_set_timer) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_swire_timer) for drv_sys_cfg_sel_swire_timer
    hal_swire.o(i.hal_swire_set_timer) refers to hal_timer.o(i.hal_timer_init) for hal_timer_init
    hal_swire.o(i.hal_swire_set_timer) refers to hal_timer.o(i.hal_timer_set_repeat) for hal_timer_set_repeat
    hal_swire.o(i.hal_swire_set_timer) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_swire.o(i.hal_swire_set_timer) refers to drv_swire.o(i.drv_swire_set_trig_mode) for drv_swire_set_trig_mode
    hal_swire.o(i.hal_swire_set_timer) refers to hal_swire.o(.data) for .data
    hal_swire.o(i.hal_swire_set_waveform) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_swire.o(i.hal_swire_set_waveform) refers to drv_swire.o(i.drv_swire_set_bit_time) for drv_swire_set_bit_time
    hal_swire.o(i.hal_swire_set_waveform) refers to drv_common.o(.data) for g_system_clock
    hal_system.o(i.hal_system_disable_systick) refers to drv_common.o(i.drv_common_disable_systick) for drv_common_disable_systick
    hal_system.o(i.hal_system_enable_systick) refers to drv_common.o(i.drv_common_enable_systick) for drv_common_enable_systick
    hal_system.o(i.hal_system_get_tick) refers to drv_common.o(i.drv_common_get_tick) for drv_common_get_tick
    hal_system.o(i.hal_system_idle_mode) refers to drv_common.o(i.drv_common_idle_mode) for drv_common_idle_mode
    hal_system.o(i.hal_system_init) refers to drv_pwr.o(i.drv_pwr_set_pll_clk) for drv_pwr_set_pll_clk
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_set_ahb_clk) for drv_crgu_set_ahb_clk
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_system.o(i.hal_system_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int) for drv_sys_cfg_clear_all_int
    hal_system.o(i.hal_system_init) refers to drv_common.o(i.drv_common_system_init) for drv_common_system_init
    hal_system.o(i.hal_system_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_system.o(i.hal_system_init) refers to drv_common.o(.data) for g_system_clock
    hal_system.o(i.hal_system_init) refers to drv_common.o(.data) for g_system_delay_step
    hal_system.o(i.hal_system_register_systick_cb) refers to drv_common.o(i.drv_common_systick_register_cb) for drv_common_systick_register_cb
    hal_system.o(i.hal_system_reset_chip) refers to drv_crgu.o(i.drv_crgu_reset_chip) for drv_crgu_reset_chip
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_set_repeat) for drv_timer_set_repeat
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_timer.o(i.hal_timer_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_timer.o(i.hal_timer_get_status) refers to drv_timer.o(i.drv_timer_get_status) for drv_timer_get_status
    hal_timer.o(i.hal_timer_init) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_timer.o(i.hal_timer_init) refers to drv_timer.o(i.drv_timer_set_prescaler) for drv_timer_set_prescaler
    hal_timer.o(i.hal_timer_set_repeat) refers to drv_timer.o(i.drv_timer_set_repeat) for drv_timer_set_repeat
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_wdg.o(i.hal_wdg_deinit) refers to drv_wdg.o(i.drv_wdg_set_int) for drv_wdg_set_int
    hal_wdg.o(i.hal_wdg_deinit) refers to drv_wdg.o(i.drv_wdg_set_repeat) for drv_wdg_set_repeat
    hal_wdg.o(i.hal_wdg_deinit) refers to drv_wdg.o(i.drv_wdg_enable) for drv_wdg_enable
    hal_wdg.o(i.hal_wdg_deinit) refers to drv_wdg.o(i.drv_wdg_register_callback) for drv_wdg_register_callback
    hal_wdg.o(i.hal_wdg_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_wdg.o(i.hal_wdg_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_wdg.o(i.hal_wdg_init) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_wdg.o(i.hal_wdg_kick_dog) refers to drv_wdg.o(i.drv_wdg_set_int) for drv_wdg_set_int
    hal_wdg.o(i.hal_wdg_kick_dog) refers to drv_wdg.o(i.drv_wdg_clear_counter) for drv_wdg_clear_counter
    hal_wdg.o(i.hal_wdg_register_callback) refers to drv_wdg.o(i.drv_wdg_register_callback) for drv_wdg_register_callback
    hal_wdg.o(i.hal_wdg_set_repeat) refers to drv_wdg.o(i.drv_wdg_set_repeat) for drv_wdg_set_repeat
    hal_wdg.o(i.hal_wdg_start) refers to drv_wdg.o(i.drv_wdg_enable) for drv_wdg_enable
    hal_wdg.o(i.hal_wdg_start) refers to drv_wdg.o(i.drv_wdg_sel_mode) for drv_wdg_sel_mode
    hal_wdg.o(i.hal_wdg_start) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_wdg.o(i.hal_wdg_start) refers to drv_wdg.o(i.drv_wdg_load_match) for drv_wdg_load_match
    hal_wdg.o(i.hal_wdg_start) refers to drv_wdg.o(i.drv_wdg_set_int) for drv_wdg_set_int
    hal_wdg.o(i.hal_wdg_stop) refers to drv_wdg.o(i.drv_wdg_set_int) for drv_wdg_set_int
    hal_wdg.o(i.hal_wdg_stop) refers to drv_wdg.o(i.drv_wdg_clear_counter) for drv_wdg_clear_counter
    hal_wdg.o(i.hal_wdg_stop) refers to drv_wdg.o(i.drv_wdg_enable) for drv_wdg_enable
    hal_crc.o(i.hal_crc_cal) refers to drv_crc.o(i.drv_crc_get_tcrc_register) for drv_crc_get_tcrc_register
    hal_crc.o(i.hal_crc_cal) refers to drv_crc.o(i.drv_crc_get_idr_counter) for drv_crc_get_idr_counter
    hal_crc.o(i.hal_crc_cal) refers to drv_crc.o(i.drv_crc_write_data_register) for drv_crc_write_data_register
    hal_crc.o(i.hal_crc_cal) refers to drv_crc.o(i.drv_crc_get_data_register) for drv_crc_get_data_register
    hal_crc.o(i.hal_crc_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_crc.o(i.hal_crc_dma_callback) refers to drv_crc.o(i.drv_crc_get_idr_counter) for drv_crc_get_idr_counter
    hal_crc.o(i.hal_crc_dma_callback) refers to drv_crc.o(i.drv_crc_get_data_register) for drv_crc_get_data_register
    hal_crc.o(i.hal_crc_dma_callback) refers to drv_crc.o(i.drv_crc_dma_disable) for drv_crc_dma_disable
    hal_crc.o(i.hal_crc_dma_callback) refers to hal_crc.o(.data) for .data
    hal_crc.o(i.hal_crc_dma_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_crc.o(i.hal_crc_dma_deinit) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_crc.o(i.hal_crc_dma_deinit) refers to drv_dma.o(i.drv_dma_deinit) for drv_dma_deinit
    hal_crc.o(i.hal_crc_dma_deinit) refers to hal_crc.o(.data) for .data
    hal_crc.o(i.hal_crc_dma_init) refers to hal_crc.o(i.hal_crc_init) for hal_crc_init
    hal_crc.o(i.hal_crc_dma_init) refers to drv_dma.o(i.drv_dma_apply_handle) for drv_dma_apply_handle
    hal_crc.o(i.hal_crc_dma_init) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_crc.o(i.hal_crc_dma_init) refers to drv_crc.o(i.drv_crc_get_tcrc_register) for drv_crc_get_tcrc_register
    hal_crc.o(i.hal_crc_dma_init) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    hal_crc.o(i.hal_crc_dma_init) refers to drv_dma.o(i.drv_dma_enable_int) for drv_dma_enable_int
    hal_crc.o(i.hal_crc_dma_init) refers to drv_dma.o(i.drv_dma_register_callback) for drv_dma_register_callback
    hal_crc.o(i.hal_crc_dma_init) refers to drv_dma.o(i.drv_dma_enable) for drv_dma_enable
    hal_crc.o(i.hal_crc_dma_init) refers to hal_crc.o(.data) for .data
    hal_crc.o(i.hal_crc_dma_init) refers to hal_crc.o(i.hal_crc_dma_callback) for hal_crc_dma_callback
    hal_crc.o(i.hal_crc_dma_start) refers to drv_crc.o(i.drv_crc_dma_enable) for drv_crc_dma_enable
    hal_crc.o(i.hal_crc_init) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_crc.o(i.hal_crc_init) refers to drv_crc.o(i.drv_crc_set_tcrc_register) for drv_crc_set_tcrc_register
    hal_crc.o(i.hal_crc_init) refers to drv_crc.o(i.drv_crc_set_initial_seed_register) for drv_crc_set_initial_seed_register
    hal_crc.o(i.hal_crc_init) refers to drv_crc.o(i.drv_crc_set_polynomial_register) for drv_crc_set_polynomial_register
    hal_crc.o(i.hal_crc_init) refers to drv_crc.o(i.drv_crc_set_rev_in_register) for drv_crc_set_rev_in_register
    hal_crc.o(i.hal_crc_init) refers to drv_crc.o(i.drv_crc_set_rev_out_register) for drv_crc_set_rev_out_register
    hal_crc.o(i.hal_crc_init) refers to drv_crc.o(i.drv_crc_set_fxor_register) for drv_crc_set_fxor_register
    hal_crc.o(i.hal_crc_init) refers to drv_crc.o(i.drv_crc_reset) for drv_crc_reset
    hal_crc.o(i.hal_crc_reset) refers to drv_crc.o(i.drv_crc_reset) for drv_crc_reset
    hal_pwr.o(i.hal_pwr_elvcc_close) refers to drv_pwr.o(i.drv_pwr_pwmled_electric_current) for drv_pwr_pwmled_electric_current
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_pwmled_electric_current) for drv_pwr_pwmled_electric_current
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_hv_ldo_mode_sel) for drv_pwr_hv_ldo_mode_sel
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_hv_ldo_mode_clock_sel) for drv_pwr_hv_ldo_mode_clock_sel
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_pwmled_driver_current_Big_step) for drv_pwr_pwmled_driver_current_Big_step
    hal_pwr.o(i.hal_pwr_elvcc_vol_set) refers to drv_pwr.o(i.drv_pwr_hv_ldo_voltage_set) for drv_pwr_hv_ldo_voltage_set
    hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode) refers to drv_pwr.o(i.drv_pwr_set_wakeup_type) for drv_pwr_set_wakeup_type
    hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode) for drv_pwr_enter_deep_sleep_mode
    hal_pwr.o(i.hal_pwr_enter_normal_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_sleep_mode_ex) for drv_pwr_enter_sleep_mode_ex
    hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_stop_sleep_mode) for drv_pwr_enter_stop_sleep_mode
    hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) refers to hal_pwr.o(.data) for .data
    hal_pwr.o(i.hal_pwr_exit_sleep_mode) refers to drv_pwr.o(i.drv_pwr_exit_sleep_mode) for drv_pwr_exit_sleep_mode
    hal_pwr.o(i.hal_pwr_get_reset_flag) refers to drv_crgu.o(i.drv_crgu_get_all_reset_flag) for drv_crgu_get_all_reset_flag
    hal_pwr.o(i.hal_pwr_get_reset_flag) refers to drv_pwr.o(i.drv_pwr_get_wakeflag) for drv_pwr_get_wakeflag
    hal_pwr.o(i.hal_pwr_get_reset_flag) refers to drv_crgu.o(i.drv_crgu_clear_all_reset_flags) for drv_crgu_clear_all_reset_flags
    hal_pwr.o(i.hal_pwr_get_vcc_power_ready) refers to drv_pwr.o(i.drv_pwr_get_power_ready_st) for drv_pwr_get_power_ready_st
    hal_pwr.o(i.hal_pwr_ldo13s_en) refers to drv_pwr.o(i.drv_pwr_ldo13s_en) for drv_pwr_ldo13s_en
    hal_pwr.o(i.hal_pwr_ldo13s_set) refers to drv_pwr.o(i.drv_pwr_ldo13s_set) for drv_pwr_ldo13s_set
    hal_pwr.o(i.hal_pwr_ldo18s_en) refers to drv_pwr.o(i.drv_pwr_ldo18s_en) for drv_pwr_ldo18s_en
    hal_pwr.o(i.hal_pwr_ldo18s_set) refers to drv_pwr.o(i.drv_pwr_ldo18s_set) for drv_pwr_ldo18s_set
    hal_pwr.o(i.hal_pwr_set_main_power) refers to drv_pwr.o(i.drv_pwr_set_digit_power_sel) for drv_pwr_set_digit_power_sel
    hal_pwr.o(i.hal_pwr_set_sleep_mode_power) refers to drv_pwr.o(i.drv_pwr_set_breath_screen_power_sel) for drv_pwr_set_breath_screen_power_sel
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_ctrl_eint) for hal_gpio_ctrl_eint
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_init_eint) for hal_gpio_init_eint
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_reg_eint_cb) for hal_gpio_reg_eint_cb
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_pwr.o(.data) for .data
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_pwr.o(i.stop_sleep_cb) for stop_sleep_cb
    hal_pwr.o(i.hal_pwr_set_vcc_enable) refers to drv_pwr.o(i.drv_pwr_charge_pump_en) for drv_pwr_charge_pump_en
    hal_pwr.o(i.stop_sleep_cb) refers to hal_pwr.o(.data) for .data
    tau_delay.o(i.delayMs) refers to tau_delay.o(i.delayUs) for delayUs
    tau_delay.o(i.delayUs) refers to drv_common.o(.data) for g_system_delay_step
    tau_log.o(i.fgetc) refers to hal_uart.o(i.hal_uart_recv_blocking) for hal_uart_recv_blocking
    tau_log.o(i.fgetc) refers to hal_system.o(i.hal_system_get_debug_state) for hal_system_get_debug_state
    tau_log.o(i.fgetc) refers to hal_system.o(i.hal_system_clear_debug_state) for hal_system_clear_debug_state
    tau_log.o(i.fgetc) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.fputc) refers to tau_log.o(i.tau_log_push_log) for tau_log_push_log
    tau_log.o(i.fputc) refers to hal_uart.o(i.hal_uart_send_blocking) for hal_uart_send_blocking
    tau_log.o(i.fputc) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.tau_log_init) refers to hal_uart.o(i.hal_uart_init) for hal_uart_init
    tau_log.o(i.tau_log_init) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.tau_log_printf) refers to memseta.o(.text) for __aeabi_memclr4
    tau_log.o(i.tau_log_printf) refers to strlen.o(.text) for strlen
    tau_log.o(i.tau_log_printf) refers to printfa.o(i.__0vsprintf) for vsprintf
    tau_log.o(i.tau_log_printf) refers to tau_log.o(i.tau_log_push_log) for tau_log_push_log
    tau_log.o(i.tau_log_printf) refers to printfa.o(i.__0printf) for __2printf
    tau_log.o(i.tau_log_printf) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.tau_log_printf) refers to tau_log.o(.bss) for g_log_buf
    tau_log.o(i.tau_log_push_log) refers to memcpya.o(.text) for __aeabi_memcpy
    tau_log.o(i.tau_log_push_log) refers to tau_delay.o(i.delayUs) for delayUs
    tau_log.o(.ARM.__at_0x1101C) refers to tau_log.o(.bss) for g_log_buf
    hal_uart.o(i.hal_uart0_rx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart0_tx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart1_rx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart1_tx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_deinit) refers to drv_uart.o(i.drv_uart_deinit) for drv_uart_deinit
    hal_uart.o(i.hal_uart_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_uart.o(i.hal_uart_deinit) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_dma_path_close) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_uart.o(i.hal_uart_dma_path_close) refers to drv_dma.o(i.drv_dma_deinit) for drv_dma_deinit
    hal_uart.o(i.hal_uart_dma_path_close) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_apply_handle) for drv_dma_apply_handle
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_set_burst) for drv_dma_set_burst
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_register_callback) for drv_dma_register_callback
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_enable_int) for drv_dma_enable_int
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_set_mem_trans_info) for drv_dma_set_mem_trans_info
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_enable) for drv_dma_enable
    hal_uart.o(i.hal_uart_dma_recv) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_uart.o(i.hal_uart_dma_recv) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_dma_recv) refers to hal_uart.o(i.hal_uart0_rx_dma_cb) for hal_uart0_rx_dma_cb
    hal_uart.o(i.hal_uart_dma_recv) refers to hal_uart.o(i.hal_uart1_rx_dma_cb) for hal_uart1_rx_dma_cb
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_apply_handle) for drv_dma_apply_handle
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_set_burst) for drv_dma_set_burst
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_register_callback) for drv_dma_register_callback
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_enable_int) for drv_dma_enable_int
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_set_mem_trans_info) for drv_dma_set_mem_trans_info
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_enable) for drv_dma_enable
    hal_uart.o(i.hal_uart_dma_send) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_uart.o(i.hal_uart_dma_send) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_dma_send) refers to hal_uart.o(i.hal_uart0_tx_dma_cb) for hal_uart0_tx_dma_cb
    hal_uart.o(i.hal_uart_dma_send) refers to hal_uart.o(i.hal_uart1_tx_dma_cb) for hal_uart1_tx_dma_cb
    hal_uart.o(i.hal_uart_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_uart.o(i.hal_uart_init) refers to drv_uart.o(i.drv_uart_init) for drv_uart_init
    hal_uart.o(i.hal_uart_init) refers to drv_uart.o(i.drv_uart_trans_create_handle) for drv_uart_trans_create_handle
    hal_uart.o(i.hal_uart_init) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_init) refers to drv_common.o(.data) for g_system_clock
    hal_uart.o(i.hal_uart_init) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_recv_blocking) refers to drv_uart.o(i.drv_uart_recv_blocking) for drv_uart_recv_blocking
    hal_uart.o(i.hal_uart_recv_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_recv_none_blocking) refers to drv_uart.o(i.drv_uart_recv_none_blocking) for drv_uart_recv_none_blocking
    hal_uart.o(i.hal_uart_recv_none_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_send_blocking) refers to drv_uart.o(i.drv_uart_send_blocking) for drv_uart_send_blocking
    hal_uart.o(i.hal_uart_send_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_send_none_blocking) refers to drv_uart.o(i.drv_uart_send_none_blocking) for drv_uart_send_none_blocking
    hal_uart.o(i.hal_uart_send_none_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_internal_vsync.o(i.LCDC_IRQn_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.LCDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_internal_vsync.o(i.LCDC_IRQn_Handler) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) for hal_intl_fb_cal_fb_info
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) for hal_dsi_tx_ctrl_gen_a_tear_signal
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_delay.o(i.delayUs) for delayUs
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) for hal_vsync_reset_lcdc_scaler
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_sync_register_rx_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) for hal_intl_fb_set_fb_info_manual
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) for hal_intl_fb_cal_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_svs.o(i.hal_intl_svs_init_rx) for hal_intl_svs_init_rx
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr) for hal_intl_dcs_init_sw_fltr
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_rxbr.o(i.drv_rxbr_register_irq1_callback) for drv_rxbr_register_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_vidc.o(i.drv_vidc_register_callback) for drv_vidc_register_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_init) for dcs_packet_fifo_init
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_gen_te) for soft_gen_te
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_gen_te_double_buffer) for soft_gen_te_double_buffer
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.rxbr_irq1_callback) for rxbr_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.vidc_callback) for vidc_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) for hal_intl_fb_cal_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_svs.o(i.hal_intl_svs_deinit_rx) for hal_intl_svs_deinit_rx
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_svs.o(i.hal_intl_svs_set_sync_coef) for hal_intl_svs_set_sync_coef
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_memc.o(i.drv_memc_set_frame_drop_select) for drv_memc_set_frame_drop_select
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_set_tear_line) for drv_lcdc_set_tear_line
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_config_acc_command_mode) for drv_lcdc_config_acc_command_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_svs.o(i.hal_intl_svs_deinit_tx) for hal_intl_svs_deinit_tx
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_svs.o(i.hal_intl_svs_set_input_frate) for hal_intl_svs_set_input_frate
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg) for drv_rxbr_hline_rcv0_cfg
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dadd.o(.text) for __aeabi_dadd
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_int_source) for drv_rxbr_get_int_source
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.soft_double_buffer_update) for soft_double_buffer_update
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_svs.o(i.hal_intl_svs_handle) for hal_intl_svs_handle
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.vpre_err_reset) for vpre_err_reset
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_lcdc.o(i.drv_lcdc_cmd_start) for drv_lcdc_cmd_start
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt) for hal_intl_svs_set_rx_vtt
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.soft_double_buffer_update) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_gen_te_double_buffer) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_get_int_source) for drv_vidc_get_int_source
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_clear_irq) for drv_vidc_clear_irq
    hal_internal_vsync.o(i.vidc_callback) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_get_irq_status) for drv_vidc_get_irq_status
    hal_internal_vsync.o(i.vidc_callback) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.vpre_err_reset) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.vpre_err_reset) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to hal_internal_dcs.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) for hal_intl_dcs_rx_receive_packet
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_dsc_dec.o(i.drv_dsc_dec_get_nslc) for drv_dsc_dec_get_nslc
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_crgu.o(i.drv_crgu_set_dsc_clk) for drv_crgu_set_dsc_clk
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to hal_internal_dcs.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr) refers to hal_internal_dcs.o(.bss) for .bss
    hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_register_write_cmd_entry) refers to hal_internal_dcs.o(.data) for .data
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle) for hal_intl_dcs_sw_filter_handle
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) for dcs_packet_fifo_alloc
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) for hal_dsi_rx_ctrl_dcs_async_handler
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_ddi_crc_en) for drv_dsi_rx_get_ddi_crc_en
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_dcs.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_dcs.o(.data) for .data
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_dcs.o(.conststring) for .conststring
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) for hal_intl_dcs_rx_get_dcs_packet_data
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) for hal_intl_dcs_rx_receive_pps
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to hal_internal_dcs.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to hal_internal_dcs.o(.conststring) for .conststring
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) refers to memseta.o(.text) for __aeabi_memset
    hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) refers to drv_rxbr.o(i.drv_rxbr_set_filter_regs) for drv_rxbr_set_filter_regs
    hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) refers to hal_internal_dcs.o(.bss) for .bss
    hal_internal_dcs.o(i.hal_intl_dcs_set_dcs_direct_mode) refers to hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) for hal_intl_dcs_set_auto_hw_filter
    hal_internal_dcs.o(i.hal_intl_dcs_set_dcs_direct_mode) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle) refers to hal_internal_dcs.o(.data) for .data
    hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle) refers to hal_internal_dcs.o(.bss) for .bss
    hal_internal_dcs.o(.data) refers to hal_internal_dcs.o(.bss) for g_imm_buffer
    hal_internal_fb.o(i.ha_intl_fb_check_pu_size) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.ha_intl_fb_check_pu_size) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter) for hal_intl_fb_flow_control_adapter
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) for hal_intl_fb_check_bandwidth
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.ha_intl_fb_check_pu_size) for ha_intl_fb_check_pu_size
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.hal_intl_fb_edge_resize) for hal_intl_fb_edge_resize
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_fb.o(i.hal_intl_fb_edge_resize) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.hal_intl_fb_edge_resize) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_user_flow) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to hal_internal_fb.o(.conststring) for .conststring
    hal_internal_svs.o(i.hal_intl_svs_deinit_rx) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.hal_intl_svs_deinit_rx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_deinit_rx) refers to hal_internal_svs.o(i.svs_wait_start) for svs_wait_start
    hal_internal_svs.o(i.hal_intl_svs_deinit_tx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_handle) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) for hal_intl_svs_update_rxbr_clk
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_svs.o(i.svs_wait_start) for svs_wait_start
    hal_internal_svs.o(i.hal_intl_svs_init_tx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_svs.o(i.svs_wait_start) for svs_wait_start
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_svs.o(i.svs_wait_fr_stab) for svs_wait_fr_stab
    hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_set_sync_coef) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to dmul.o(.text) for __aeabi_dmul
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg) for drv_rxbr_hline_rcv1_cfg
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_get_rel_intv) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_svs.o(i.svs_get_rel_intv) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_sync_handle) refers to hal_internal_svs.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_svs.o(i.svs_sync_handle) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_svs.o(i.svs_sync_handle) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_svs.o(i.svs_sync_handle) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_svs.o(i.svs_sync_handle) refers to f2d.o(.text) for __aeabi_f2d
    hal_internal_svs.o(i.svs_sync_handle) refers to dadd.o(.text) for __aeabi_dadd
    hal_internal_svs.o(i.svs_sync_handle) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_svs.o(i.svs_sync_handle) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to hal_internal_svs.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to ffixui.o(.text) for __aeabi_f2uiz
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to hal_internal_svs.o(i.svs_sync_handle) for svs_sync_handle
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_svs.o(i.svs_wait_start) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_internal_svs.o(i.svs_wait_start) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_svs.o(i.svs_wait_start) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_internal_svs.o(i.svs_wait_start) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_svs.o(i.svs_wait_start) refers to f2d.o(.text) for __aeabi_f2d
    hal_internal_svs.o(i.svs_wait_start) refers to ceil.o(i.ceil) for ceil
    hal_internal_svs.o(i.svs_wait_start) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(i.svs_direct_mode_setting) for svs_direct_mode_setting
    hal_internal_svs.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_svs.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg) for drv_rxbr_hline_rcv1_cfg
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(i.svs_wait_fr_stab) for svs_wait_fr_stab
    drv_common.o(i.HardFault_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_common.o(i.SysTick_Handler) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_enable_systick) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_common.o(i.drv_common_enable_systick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_get_tick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_system_init) refers to drv_se.o(i.drv_se_init) for drv_se_init
    drv_common.o(i.drv_common_systick_register_cb) refers to drv_common.o(.data) for .data
    drv_crgu.o(i.drv_crgu_get_rxbr_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_crgu.o(i.drv_crgu_get_system_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(i.drv_dma_get_int_source) for drv_dma_get_int_source
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(i.drv_dma_clear_status) for drv_dma_clear_status
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(.data) for .data
    drv_dma.o(i.drv_dma_apply_handle) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dma.o(i.drv_dma_apply_handle) refers to drv_dma.o(.data) for .data
    drv_dma.o(i.drv_dma_apply_handle) refers to drv_dma.o(.constdata) for .constdata
    drv_dma.o(i.drv_dma_deinit) refers to drv_dma.o(i.drv_dma_disable_int) for drv_dma_disable_int
    drv_dma.o(i.drv_dma_disable_int) refers to drv_dma.o(i.drv_dma_int_list_delete) for drv_dma_int_list_delete
    drv_dma.o(i.drv_dma_disable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.drv_dma_enable_int) refers to drv_dma.o(i.drv_dma_int_list_inset) for drv_dma_int_list_inset
    drv_dma.o(i.drv_dma_enable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dma.o(i.drv_dma_init) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    drv_dma.o(i.drv_dma_init) refers to drv_dma.o(i.drv_dma_update_handle_setting) for drv_dma_update_handle_setting
    drv_dma.o(i.drv_dma_int_list_delete) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_int_list_inset) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_update_handle_setting) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_dma_req) for drv_sys_cfg_sel_dma_req
    drv_dma.o(i.drv_dma_update_req_by_default) refers to drv_dma.o(i.drv_dma_update_handle_setting) for drv_dma_update_handle_setting
    drv_dma.o(i.drv_dma_update_req_by_default) refers to drv_dma.o(.constdata) for .constdata
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to drv_se.o(i.drv_se_set_dsc) for drv_se_set_dsc
    drv_gpio.o(i.AP_NRESET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.AP_NRESET_IRQn_Handler) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.EXTI_INT0_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT1_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT2_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT3_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT4_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT5_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT6_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT7_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.drv_gpio_handle_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.drv_gpio_handle_int) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_register_ap_reset_callback) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.drv_gpio_register_callback) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_pwr.o(i.drv_pwr_analog_pwm_en) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_elvcc_pwm_en) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_elvcc_pwm_en) refers to tau_delay.o(i.delayMs) for delayMs
    drv_pwr.o(i.drv_pwr_enter_sleep_mode) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_enter_sleep_mode) refers to drv_pwr.o(i.drv_pwr_por_mode_flag) for drv_pwr_por_mode_flag
    drv_pwr.o(i.drv_pwr_enter_stop_sleep_mode) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_exit_sleep_mode) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_hv_ldo_mode_clock_sel) refers to drv_pwr.o(i.drv_pwr_hv_ldo_10M_clock) for drv_pwr_hv_ldo_10M_clock
    drv_pwr.o(i.drv_pwr_pwm_output_pwm_led) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_breath_screen_power_sel) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_digit_power_sel) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_system_clk) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_wakeup_type) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_spi_master.o(i.drv_spim_disable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_spi_master.o(i.drv_spim_disable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_spi_master.o(i.drv_spim_enable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_spi_master.o(i.drv_spim_enable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_spi_master.o(i.drv_spim_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_spi_master.o(i.drv_spim_init) refers to drv_common.o(.data) for g_system_clock
    drv_spi_master.o(i.drv_spim_read) refers to drv_spi_master.o(i.drv_spim_flush) for drv_spim_flush
    drv_spi_master.o(i.drv_spim_register_callback) refers to drv_spi_master.o(.data) for .data
    drv_spi_master.o(i.drv_spim_write) refers to drv_spi_master.o(i.drv_spim_get_busy) for drv_spim_get_busy
    drv_spi_master.o(i.drv_spim_write) refers to drv_spi_master.o(i.drv_spim_flush) for drv_spim_flush
    drv_swire.o(i.SWIRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_swire.o(i.SWIRE_IRQn_Handler) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_register_callback) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_sys_cfg.o(i.drv_sys_cfg_sel_dma_req) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_timer.o(i.TIMER0_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.TIMER1_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.TIMER2_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.TIMER3_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_timer.o(i.drv_timer_enable) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_get_instance) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_get_status) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_clear_status_flags) for drv_timer_clear_status_flags
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_register_callback) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_compare_val) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_compare_val) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_timer.o(i.drv_timer_set_compare_val) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_compare_val) refers to drv_common.o(.data) for g_system_clock
    drv_timer.o(i.drv_timer_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_repeat) refers to drv_timer.o(.data) for .data
    drv_wdg.o(i.WDG_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_wdg.o(i.WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_set_int) for drv_wdg_set_int
    drv_wdg.o(i.WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_clear_counter) for drv_wdg_clear_counter
    drv_wdg.o(i.WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_read_edge_flag) for drv_wdg_read_edge_flag
    drv_wdg.o(i.WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_clear_edge_flag) for drv_wdg_clear_edge_flag
    drv_wdg.o(i.WDG_IRQn_Handler) refers to drv_wdg.o(.data) for .data
    drv_wdg.o(i.drv_wdg_register_callback) refers to drv_wdg.o(.data) for .data
    drv_wdg.o(i.drv_wdg_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_wdg.o(i.drv_wdg_set_repeat) refers to drv_wdg.o(.data) for .data
    drv_crc.o(i.drv_crc_write_data_register) refers to drv_crc.o(i.drv_crc_get_tcrc_register) for drv_crc_get_tcrc_register
    drv_i2c.o(i.I2C0_IRQn_Handler) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.I2C1_IRQn_Handler) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.I2C2_IRQn_Handler) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_NVIC_enable) refers to drv_i2c.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_i2c.o(i.drv_i2c_NVIC_enable) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_clear_intr_status) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_i2c.o(i.drv_i2c_clear_intr_status) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_clock_enable) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    drv_i2c.o(i.drv_i2c_clock_enable) refers to drv_i2c.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_i2c.o(i.drv_i2c_clock_enable) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_i2c.o(i.drv_i2c_clock_enable) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_disable_dma_req) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_disable_intr) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_enable) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_enable_dma_req) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_enable_intr) refers to drv_i2c.o(i.drv_i2c_set_sys_mask) for drv_i2c_set_sys_mask
    drv_i2c.o(i.drv_i2c_enable_intr) refers to drv_i2c.o(i.drv_i2c_clear_intr_status) for drv_i2c_clear_intr_status
    drv_i2c.o(i.drv_i2c_enable_intr) refers to drv_i2c.o(i.drv_i2c_NVIC_enable) for drv_i2c_NVIC_enable
    drv_i2c.o(i.drv_i2c_enable_intr) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_flush) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_get_fifo_status) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_get_intr_status) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_get_rx_count) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_get_tx_abrtsource) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_read_data) refers to drv_i2c.o(i.drv_i2c_get_fifo_status) for drv_i2c_get_fifo_status
    drv_i2c.o(i.drv_i2c_read_data) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_set_callback) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_set_fifo_threshold) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_set_sys_mask) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_i2c.o(i.drv_i2c_set_sys_mask) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_i2c.o(i.drv_i2c_set_sys_mask) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_write_data) refers to drv_i2c.o(i.drv_i2c_get_fifo_status) for drv_i2c_get_fifo_status
    drv_i2c.o(i.drv_i2c_write_data) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cm_cal_scl_cnt) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_i2c.o(i.drv_i2cm_cal_scl_cnt) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cm_init) refers to drv_i2c.o(i.drv_i2cm_cal_scl_cnt) for drv_i2cm_cal_scl_cnt
    drv_i2c.o(i.drv_i2cm_init) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cm_init) refers to drv_common.o(.data) for g_system_clock
    drv_i2c.o(i.drv_i2cm_read_data) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cm_set_baud_rate) refers to drv_i2c.o(i.drv_i2cm_cal_scl_cnt) for drv_i2cm_cal_scl_cnt
    drv_i2c.o(i.drv_i2cm_set_baud_rate) refers to drv_common.o(.data) for g_system_clock
    drv_i2c.o(i.drv_i2cm_set_baud_rate) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cm_set_slave_addr) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cm_write_data) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cm_write_read_cmd) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cs_init) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cs_own_addr) refers to drv_i2c.o(.data) for .data
    dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_fifo_init) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_size) refers to dcs_packet_fifo.o(.bss) for .bss
    drv_se.o(i.drv_se_init) refers to drv_efuse.o(i.drv_efuse_enter_inactive) for drv_efuse_enter_inactive
    drv_se.o(i.drv_se_init) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_se.o(i.drv_se_init) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_dsc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_dsc) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_lcdc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_lcdc) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_memc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_memc) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_rxbr) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_rxbr) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_vidc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_vidc) refers to drv_se.o(.data) for .data
    drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) refers to drv_dsi_rx.o(.data) for .data
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) for drv_dsi_rx_get_color_bpp
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to ffltui.o(.text) for __aeabi_ui2f
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fdiv.o(.text) for __aeabi_fdiv
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fmul.o(.text) for __aeabi_fmul
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc) for drv_dsi_rx_get_color_pcc
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fadd.o(.text) for __aeabi_fadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to cfrcmple.o(.text) for __aeabi_cfrcmple
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to f2d.o(.text) for __aeabi_f2d
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dadd.o(.text) for __aeabi_dadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dfixui.o(.text) for __aeabi_d2uiz
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_set_drv_log_level) refers to drv_dsi_rx.o(.data) for .data
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_test_lock) for drv_phy_test_lock
    drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_enter) for drv_tx_phy_test_enter
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_code) for drv_tx_phy_test_write_code
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_exit) for drv_tx_phy_test_exit
    drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_version) for drv_dsi_tx_version
    drv_dsi_tx.o(i.drv_dsi_tx_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_tx.o(i.drv_dsi_tx_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_lcdc.o(i.drv_lcdc_clear_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_lcdc.o(i.drv_lcdc_cmd_start) refers to drv_se.o(i.drv_se_set_lcdc) for drv_se_set_lcdc
    drv_lcdc.o(i.drv_lcdc_ctrl_flow) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    drv_lcdc.o(i.drv_lcdc_part_display_config) refers to drv_lcdc.o(i.drv_lcdc_pixel_value_config) for drv_lcdc_pixel_value_config
    drv_lcdc.o(i.drv_lcdc_set_int) refers to drv_lcdc.o(i.drv_lcdc_clear_int) for drv_lcdc_clear_int
    drv_lcdc.o(i.drv_lcdc_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_lcdc.o(i.drv_lcdc_vid_hw_start) refers to drv_se.o(i.drv_se_set_lcdc) for drv_se_set_lcdc
    drv_memc.o(i.MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_get_status) for drv_memc_get_status
    drv_memc.o(i.MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_clear_status) for drv_memc_clear_status
    drv_memc.o(i.MEMC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_memc.o(i.drv_memc_rate_transfer_sel) refers to drv_se.o(i.drv_se_set_memc) for drv_se_set_memc
    drv_memc.o(i.drv_memc_set_ltpo_mode) refers to drv_se.o(i.drv_se_set_memc) for drv_se_set_memc
    drv_rxbr.o(i.VPRE1_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.VPRE1_IRQn_Handler) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_EnableIRQ) for __NVIC_EnableIRQ
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_rxbr.o(i.drv_rxbr_register_irq0_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_register_irq1_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_set_cmd_filter) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_rxbr.o(i.drv_rxbr_set_cmd_response) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_rxbr.o(i.drv_rxbr_set_color_format) refers to drv_se.o(i.drv_se_set_rxbr) for drv_se_set_rxbr
    drv_rxbr.o(i.drv_rxbr_soft_reset) refers to tau_delay.o(i.delayMs) for delayMs
    drv_vidc.o(i.VIDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.VIDC_IRQn_Handler) refers to drv_vidc.o(.data) for .data
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_vidc.o(i.drv_vidc_register_callback) refers to drv_vidc.o(.data) for .data
    drv_vidc.o(i.drv_vidc_set_src_parameter) refers to drv_se.o(i.drv_se_set_vidc) for drv_se_set_vidc
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_int_trans_handle) for drv_uart_int_trans_handle
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_abort_recv) for drv_uart_abort_recv
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_abort_send) for drv_uart_abort_send
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(.constdata) for .constdata
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(i.drv_uart_reset_rx_fifo) for drv_uart_reset_rx_fifo
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(i.drv_uart_reset_tx_fifo) for drv_uart_reset_tx_fifo
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_deinit) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_deinit) refers to drv_uart.o(i.drv_uart_enable_clk) for drv_uart_enable_clk
    drv_uart.o(i.drv_uart_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.drv_uart_deinit) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_enable_clk) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    drv_uart.o(i.drv_uart_enable_int) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_enable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.drv_uart_get_def_cfg) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.drv_uart_get_def_cfg) refers to drv_common.o(.data) for g_system_clock
    drv_uart.o(i.drv_uart_get_instance) refers to drv_uart.o(.constdata) for .constdata
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_enable_clk) for drv_uart_enable_clk
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_set_baud_rate) for drv_uart_set_baud_rate
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_enable_int) for drv_uart_enable_int
    drv_uart.o(i.drv_uart_int_trans_handle) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_recv_none_blocking) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_recv_none_blocking) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_recv_none_blocking) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_reset_rx_fifo) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_reset_tx_fifo) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_send_none_blocking) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_send_none_blocking) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_send_none_blocking) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_set_baud_rate) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_uart.o(i.drv_uart_trans_create_handle) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_trans_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.drv_uart_trans_create_handle) refers to drv_uart.o(.bss) for .bss
    drv_efuse.o(i.drv_efuse_enter_inactive) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    drv_efuse.o(i.drv_efuse_enter_inactive) refers to drv_efuse.o(i.drv_efuse_int_enable) for drv_efuse_int_enable
    drv_efuse.o(i.drv_efuse_read) refers to drv_pwr.o(i.drv_pwr_efuse_pd) for drv_pwr_efuse_pd
    drv_efuse.o(i.drv_efuse_read) refers to drv_efuse.o(i.drv_efuse_read_req) for drv_efuse_read_req
    drv_efuse.o(i.drv_efuse_write) refers to drv_pwr.o(i.drv_pwr_efuse_pd) for drv_pwr_efuse_pd
    drv_efuse.o(i.drv_efuse_write) refers to drv_efuse.o(i.drv_efuse_write_req) for drv_efuse_write_req
    drv_efuse.o(i.drv_efuse_write_read_req_clear) refers to drv_efuse.o(i.drv_efuse_write_req) for drv_efuse_write_req
    drv_efuse.o(i.drv_efuse_write_read_req_clear) refers to drv_efuse.o(i.drv_efuse_read_req) for drv_efuse_read_req
    ceil.o(i.__softfp_ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.__softfp_ceil) refers to ceil.o(i.ceil) for ceil
    ceil.o(i.ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.ceil) refers to dadd.o(.text) for __aeabi_dadd
    ceil.o(i.ceil) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry10a.o(.ARM.Collect$$$$0000000D) for __rt_final_cpp
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry11a.o(.ARM.Collect$$$$0000000F) for __rt_final_exit
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry7b.o(.ARM.Collect$$$$00000008) for _main_clock
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry8b.o(.ARM.Collect$$$$0000000A) for _main_cpp_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry9a.o(.ARM.Collect$$$$0000000B) for _main_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry5.o(.ARM.Collect$$$$00000004) for _main_scatterload
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry2.o(.ARM.Collect$$$$00000001) for _main_stk
    idiv.o(.text) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfb.o(i.__0fprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0fprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0printf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printfb.o(i.__0vfprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vfprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printf0.o(i.__0fprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0fprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0printf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf0.o(i.__0vfprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vfprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf1.o(i.__0fprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0fprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0printf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i.__0vfprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vfprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf2.o(i.__0fprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0fprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0printf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf2.o(i.__0vfprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vfprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf3.o(i.__0fprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0fprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0printf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i.__0vfprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vfprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf4.o(i.__0fprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0fprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0printf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i.__0vfprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vfprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf5.o(i.__0fprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0fprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0printf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i.__0vfprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vfprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf6.o(i.__0fprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0fprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0printf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i.__0vfprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vfprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i._printf_core) refers to printf6.o(i._printf_pre_padding) for _printf_pre_padding
    printf6.o(i._printf_core) refers to printf6.o(i._printf_post_padding) for _printf_post_padding
    printf6.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf7.o(i.__0fprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0fprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0printf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i.__0vfprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vfprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i._printf_core) refers to printf7.o(i._printf_pre_padding) for _printf_pre_padding
    printf7.o(i._printf_core) refers to printf7.o(i._printf_post_padding) for _printf_post_padding
    printf7.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf8.o(i.__0fprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0fprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0printf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i.__0vfprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vfprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i._printf_core) refers to printf8.o(i._printf_pre_padding) for _printf_pre_padding
    printf8.o(i._printf_core) refers to printf8.o(i._printf_post_padding) for _printf_post_padding
    printf8.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i.__0fprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0fprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0fprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0printf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0printf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0snprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0snprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0snprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0sprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0sprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0sprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i.__0vfprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vfprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vfprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0vsnprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0vsprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i._fp_digits) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._fp_digits) refers to dmul.o(.text) for __aeabi_dmul
    printfa.o(i._fp_digits) refers to ddiv.o(.text) for __aeabi_ddiv
    printfa.o(i._fp_digits) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    printfa.o(i._fp_digits) refers to dadd.o(.text) for __aeabi_dadd
    printfa.o(i._fp_digits) refers to dfixul.o(.text) for __aeabi_d2ulz
    printfa.o(i._fp_digits) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_core) refers to printfa.o(i._printf_pre_padding) for _printf_pre_padding
    printfa.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers to printfa.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i._printf_core) refers to printfa.o(i._fp_digits) for _fp_digits
    printfa.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfa.o(i._printf_post_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_pre_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._snputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._sputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    fmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers to fepilogue.o(.text) for _float_round
    fscalb.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    dadd.o(.text) refers to llsshr.o(.text) for __aeabi_lasr
    dadd.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dmul.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ddiv.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ddiv.o(.text) refers to depilogue.o(.text) for _double_round
    ffltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ffltui.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    dfltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfltui.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ffixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixui.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    f2d.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    d2f.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    d2f.o(.text) refers to fepilogue.o(.text) for _float_round
    cfcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    cfrcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    entry2.o(.ARM.Collect$$$$00000001) refers to entry2.o(.ARM.Collect$$$$00002712) for __lit__00000000
    entry2.o(.ARM.Collect$$$$00002712) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    entry5.o(.ARM.Collect$$$$00000004) refers to init.o(.text) for __scatterload
    entry9a.o(.ARM.Collect$$$$0000000B) refers to main.o(i.main) for main
    entry9b.o(.ARM.Collect$$$$0000000C) refers to main.o(i.main) for main
    uldiv.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    uldiv.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to depilogue.o(i.__ARM_clz) for __ARM_clz
    depilogue.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixul.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixul.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    init.o(.text) refers to entry5.o(.ARM.Collect$$$$00000004) for __main_after_scatterload


==============================================================================

Removing Unused input sections from the image.

    Removing main.o(.rev16_text), (4 bytes).
    Removing main.o(.revsh_text), (4 bytes).
    Removing app_tp_transfer.o(.rev16_text), (4 bytes).
    Removing app_tp_transfer.o(.revsh_text), (4 bytes).
    Removing app_tp_transfer.o(i.app_tp_i2cs_callback), (76 bytes).
    Removing app_tp_transfer.o(i.app_tp_init), (108 bytes).
    Removing app_tp_transfer.o(i.app_tp_m_read), (24 bytes).
    Removing app_tp_transfer.o(i.app_tp_m_transfer_complate), (8 bytes).
    Removing app_tp_transfer.o(i.app_tp_m_write), (28 bytes).
    Removing app_tp_transfer.o(i.app_tp_phone_clear_reset_on), (12 bytes).
    Removing app_tp_transfer.o(i.app_tp_phone_reset_init), (60 bytes).
    Removing app_tp_transfer.o(i.app_tp_phone_reset_on), (12 bytes).
    Removing app_tp_transfer.o(i.app_tp_reset_callback), (12 bytes).
    Removing app_tp_transfer.o(i.app_tp_s_read), (20 bytes).
    Removing app_tp_transfer.o(i.app_tp_s_write), (22 bytes).
    Removing app_tp_transfer.o(i.app_tp_screen_init), (60 bytes).
    Removing app_tp_transfer.o(i.app_tp_screen_int_callback), (12 bytes).
    Removing app_tp_transfer.o(i.app_tp_screen_int_init), (64 bytes).
    Removing app_tp_transfer.o(i.app_tp_screen_int_lvl_low), (28 bytes).
    Removing app_tp_transfer.o(i.app_tp_transfer_phone), (48 bytes).
    Removing app_tp_transfer.o(i.app_tp_transfer_screen_const), (256 bytes).
    Removing app_tp_transfer.o(i.app_tp_transfer_screen_int), (368 bytes).
    Removing app_tp_transfer.o(i.app_tp_transfer_screen_start), (32 bytes).
    Removing app_tp_transfer.o(i.phone_i2cs_io_init), (28 bytes).
    Removing app_tp_transfer.o(i.screen_spim_io_init), (28 bytes).
    Removing app_tp_transfer.o(.bss), (500 bytes).
    Removing app_tp_transfer.o(.constdata), (24 bytes).
    Removing app_tp_transfer.o(.data), (28 bytes).
    Removing app_tp_for_custom_s8.o(.rev16_text), (4 bytes).
    Removing app_tp_for_custom_s8.o(.revsh_text), (4 bytes).
    Removing app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data), (528 bytes).
    Removing app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const), (80 bytes).
    Removing app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int), (1152 bytes).
    Removing app_tp_for_custom_s8.o(i.app_tp_write_other_operations), (60 bytes).
    Removing app_tp_for_custom_s8.o(.bss), (142 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (1838 bytes).
    Removing app_tp_for_custom_s8.o(.data), (687 bytes).
    Removing s8_demo.o(.rev16_text), (4 bytes).
    Removing s8_demo.o(.revsh_text), (4 bytes).
    Removing s8_demo.o(i.ap_dcs_read), (232 bytes).
    Removing s8_demo.o(i.ap_dcs_set_eye_protection_mode), (100 bytes).
    Removing s8_demo.o(i.ap_rstn_pull_down_cb), (92 bytes).
    Removing s8_demo.o(i.app_mipi_rx_start_cb), (80 bytes).
    Removing board.o(.rev16_text), (4 bytes).
    Removing board.o(.revsh_text), (4 bytes).
    Removing startup_armcm0.o(HEAP), (3072 bytes).
    Removing demo_hal_crc.o(.rev16_text), (4 bytes).
    Removing demo_hal_crc.o(.revsh_text), (4 bytes).
    Removing demo_hal_crc.o(i.demo_crc_array_dma_cal), (44 bytes).
    Removing demo_hal_crc.o(i.demo_crc_dma_callback), (60 bytes).
    Removing demo_hal_crc.o(i.demo_hal_crc_case), (60 bytes).
    Removing demo_hal_crc.o(.constdata), (12 bytes).
    Removing demo_hal_crc.o(.data), (128 bytes).
    Removing demo_hal_dsi_rx.o(.rev16_text), (4 bytes).
    Removing demo_hal_dsi_rx.o(.revsh_text), (4 bytes).
    Removing demo_hal_dsi_rx.o(i.ap_dcs_read), (220 bytes).
    Removing demo_hal_dsi_rx.o(i.cus_dsc_execute), (188 bytes).
    Removing demo_hal_dsi_rx.o(i.demo_hal_dsi_rx_case), (88 bytes).
    Removing demo_hal_dsi_rx.o(i.open_mipi_rx), (200 bytes).
    Removing demo_hal_dsi_rx.o(.constdata), (240 bytes).
    Removing demo_hal_dsi_rx.o(.data), (4 bytes).
    Removing demo_hal_dsi_tx.o(.rev16_text), (4 bytes).
    Removing demo_hal_dsi_tx.o(.revsh_text), (4 bytes).
    Removing demo_hal_dsi_tx.o(i.demo_dsi_tx_case), (68 bytes).
    Removing demo_hal_dsi_tx.o(i.demo_open_mipi_rx), (2 bytes).
    Removing demo_hal_dsi_tx.o(i.demo_open_mipi_tx), (376 bytes).
    Removing demo_hal_dsi_tx.o(i.demo_panel_init), (400 bytes).
    Removing demo_hal_dsi_tx.o(.data), (5 bytes).
    Removing demo_hal_flash.o(.rev16_text), (4 bytes).
    Removing demo_hal_flash.o(.revsh_text), (4 bytes).
    Removing demo_hal_gpio.o(.rev16_text), (4 bytes).
    Removing demo_hal_gpio.o(.revsh_text), (4 bytes).
    Removing demo_hal_i2c.o(.rev16_text), (4 bytes).
    Removing demo_hal_i2c.o(.revsh_text), (4 bytes).
    Removing demo_hal_spi.o(.rev16_text), (4 bytes).
    Removing demo_hal_spi.o(.revsh_text), (4 bytes).
    Removing demo_hal_pwm.o(.rev16_text), (4 bytes).
    Removing demo_hal_pwm.o(.revsh_text), (4 bytes).
    Removing demo_hal_pwr.o(.rev16_text), (4 bytes).
    Removing demo_hal_pwr.o(.revsh_text), (4 bytes).
    Removing demo_hal_swire.o(.rev16_text), (4 bytes).
    Removing demo_hal_swire.o(.revsh_text), (4 bytes).
    Removing demo_hal_uart.o(.rev16_text), (4 bytes).
    Removing demo_hal_uart.o(.revsh_text), (4 bytes).
    Removing demo_hal_wdg.o(.rev16_text), (4 bytes).
    Removing demo_hal_wdg.o(.revsh_text), (4 bytes).
    Removing demo_hal_wdg.o(i.demo_wdg_callback), (72 bytes).
    Removing demo_hal_wdg.o(i.demo_wdg_case), (60 bytes).
    Removing demo_hal_wdg.o(i.demo_wdg_case_int_mode), (196 bytes).
    Removing demo_hal_wdg.o(.data), (3 bytes).
    Removing module_demo_main.o(i.module_demo_main), (2 bytes).
    Removing hal_dsi_rx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd), (220 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_short_cmd), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init), (60 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern), (260 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_force_video_crtl), (12 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en), (8 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size), (32 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback), (52 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_write_cmd_entry), (10 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle), (40 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart), (68 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd), (240 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_check_crc), (24 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk), (32 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter), (44 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_log_level), (8 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data), (62 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk), (72 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk), (56 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate), (10 bytes).
    Removing hal_dsi_tx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode), (112 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_frame), (12 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_overwrite_enable), (22 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd), (128 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle), (32 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs), (44 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm), (8 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_sync_line), (36 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect), (44 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance), (44 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness), (12 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div), (8 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc), (44 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg), (18 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera), (68 bytes).
    Removing hal_gpio.o(.rev16_text), (4 bytes).
    Removing hal_gpio.o(.revsh_text), (4 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_input_data), (18 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_int_type), (20 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_pull_state), (40 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_driving_strength), (44 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_high_impedance), (44 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_schmitt_trigger), (52 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_slew_rate), (52 bytes).
    Removing hal_i2c_slave.o(.rev16_text), (4 bytes).
    Removing hal_i2c_slave.o(.revsh_text), (4 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_callback), (180 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_deinit), (44 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_get_rx_cnt), (16 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_get_tx_cnt), (16 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_get_write_complete), (20 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_init), (108 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_register_callback), (16 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_rx_cnt_clear), (20 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_start), (96 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_stop), (84 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_tx_dma_callback), (56 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer), (72 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer), (80 bytes).
    Removing hal_i2c_slave.o(.data), (144 bytes).
    Removing hal_spi_master.o(.rev16_text), (4 bytes).
    Removing hal_spi_master.o(.revsh_text), (4 bytes).
    Removing hal_spi_master.o(i.hal_spim_deinit), (16 bytes).
    Removing hal_spi_master.o(i.hal_spim_flush), (10 bytes).
    Removing hal_spi_master.o(i.hal_spim_get_transfer_complete), (12 bytes).
    Removing hal_spi_master.o(i.hal_spim_init), (40 bytes).
    Removing hal_spi_master.o(i.hal_spim_read), (56 bytes).
    Removing hal_spi_master.o(i.hal_spim_write), (48 bytes).
    Removing hal_spi_master.o(.data), (4 bytes).
    Removing hal_spi_master.o(.data), (4 bytes).
    Removing hal_swire.o(.rev16_text), (4 bytes).
    Removing hal_swire.o(.revsh_text), (4 bytes).
    Removing hal_swire.o(i.hal_swire_register_callback), (22 bytes).
    Removing hal_swire.o(i.hal_swire_set_waveform), (92 bytes).
    Removing hal_system.o(.rev16_text), (4 bytes).
    Removing hal_system.o(.revsh_text), (4 bytes).
    Removing hal_system.o(i.hal_system_clear_debug_state), (10 bytes).
    Removing hal_system.o(i.hal_system_disable_systick), (8 bytes).
    Removing hal_system.o(i.hal_system_enable_systick), (8 bytes).
    Removing hal_system.o(i.hal_system_get_debug_state), (8 bytes).
    Removing hal_system.o(i.hal_system_get_tick), (8 bytes).
    Removing hal_system.o(i.hal_system_idle_mode), (8 bytes).
    Removing hal_system.o(i.hal_system_register_systick_cb), (8 bytes).
    Removing hal_system.o(i.hal_system_reset_chip), (10 bytes).
    Removing hal_timer.o(.rev16_text), (4 bytes).
    Removing hal_timer.o(.revsh_text), (4 bytes).
    Removing hal_timer.o(i.hal_timer_get_status), (8 bytes).
    Removing hal_timer.o(i.hal_timer_start_ex), (42 bytes).
    Removing hal_wdg.o(.rev16_text), (4 bytes).
    Removing hal_wdg.o(.revsh_text), (4 bytes).
    Removing hal_wdg.o(i.hal_wdg_deinit), (44 bytes).
    Removing hal_wdg.o(i.hal_wdg_init), (12 bytes).
    Removing hal_wdg.o(i.hal_wdg_kick_dog), (20 bytes).
    Removing hal_wdg.o(i.hal_wdg_register_callback), (8 bytes).
    Removing hal_wdg.o(i.hal_wdg_set_repeat), (8 bytes).
    Removing hal_wdg.o(i.hal_wdg_start), (54 bytes).
    Removing hal_wdg.o(i.hal_wdg_stop), (20 bytes).
    Removing hal_crc.o(.rev16_text), (4 bytes).
    Removing hal_crc.o(.revsh_text), (4 bytes).
    Removing hal_crc.o(i.hal_crc_cal), (72 bytes).
    Removing hal_crc.o(i.hal_crc_deinit), (16 bytes).
    Removing hal_crc.o(i.hal_crc_dma_callback), (40 bytes).
    Removing hal_crc.o(i.hal_crc_dma_deinit), (44 bytes).
    Removing hal_crc.o(i.hal_crc_dma_init), (120 bytes).
    Removing hal_crc.o(i.hal_crc_dma_start), (10 bytes).
    Removing hal_crc.o(i.hal_crc_init), (56 bytes).
    Removing hal_crc.o(i.hal_crc_reset), (10 bytes).
    Removing hal_crc.o(.data), (8 bytes).
    Removing hal_pwr.o(.rev16_text), (4 bytes).
    Removing hal_pwr.o(.revsh_text), (4 bytes).
    Removing hal_pwr.o(i.hal_pwr_elvcc_close), (10 bytes).
    Removing hal_pwr.o(i.hal_pwr_elvcc_ldo_en), (46 bytes).
    Removing hal_pwr.o(i.hal_pwr_elvcc_vol_set), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_get_reset_flag), (66 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo13s_en), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo13s_set), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo18s_en), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo18s_set), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_set_vcc_enable), (8 bytes).
    Removing tau_delay.o(.rev16_text), (4 bytes).
    Removing tau_delay.o(.revsh_text), (4 bytes).
    Removing tau_log.o(.rev16_text), (4 bytes).
    Removing tau_log.o(.revsh_text), (4 bytes).
    Removing tau_log.o(i.fgetc), (72 bytes).
    Removing hal_uart.o(.rev16_text), (4 bytes).
    Removing hal_uart.o(.revsh_text), (4 bytes).
    Removing hal_uart.o(i.hal_uart0_rx_dma_cb), (20 bytes).
    Removing hal_uart.o(i.hal_uart0_tx_dma_cb), (36 bytes).
    Removing hal_uart.o(i.hal_uart1_rx_dma_cb), (20 bytes).
    Removing hal_uart.o(i.hal_uart1_tx_dma_cb), (36 bytes).
    Removing hal_uart.o(i.hal_uart_deinit), (48 bytes).
    Removing hal_uart.o(i.hal_uart_dma_path_close), (92 bytes).
    Removing hal_uart.o(i.hal_uart_dma_recv), (276 bytes).
    Removing hal_uart.o(i.hal_uart_dma_send), (280 bytes).
    Removing hal_uart.o(i.hal_uart_recv_blocking), (28 bytes).
    Removing hal_uart.o(i.hal_uart_recv_none_blocking), (28 bytes).
    Removing hal_uart.o(i.hal_uart_send_none_blocking), (28 bytes).
    Removing hal_internal_vsync.o(.rev16_text), (4 bytes).
    Removing hal_internal_vsync.o(.revsh_text), (4 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te), (2 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_register_rx_callback), (28 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual), (28 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line), (60 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate), (134 bytes).
    Removing hal_internal_vsync.o(.data), (4 bytes).
    Removing hal_internal_dcs.o(.rev16_text), (4 bytes).
    Removing hal_internal_dcs.o(.revsh_text), (4 bytes).
    Removing hal_internal_dcs.o(i.hal_intl_dcs_register_write_cmd_entry), (12 bytes).
    Removing hal_internal_dcs.o(i.hal_intl_dcs_set_dcs_direct_mode), (44 bytes).
    Removing hal_internal_fb.o(.rev16_text), (4 bytes).
    Removing hal_internal_fb.o(.revsh_text), (4 bytes).
    Removing hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual), (512 bytes).
    Removing hal_internal_fb.o(.conststring), (152 bytes).
    Removing hal_internal_svs.o(.rev16_text), (4 bytes).
    Removing hal_internal_svs.o(.revsh_text), (4 bytes).
    Removing hal_internal_svs.o(i.hal_intl_svs_set_input_frate), (112 bytes).
    Removing hal_internal_svs.o(i.hal_intl_svs_set_sync_coef), (12 bytes).
    Removing drv_common.o(.rev16_text), (4 bytes).
    Removing drv_common.o(.revsh_text), (4 bytes).
    Removing drv_common.o(i.drv_common_disable_systick), (20 bytes).
    Removing drv_common.o(i.drv_common_enable_systick), (88 bytes).
    Removing drv_common.o(i.drv_common_get_tick), (12 bytes).
    Removing drv_common.o(i.drv_common_idle_mode), (40 bytes).
    Removing drv_common.o(i.drv_common_systick_register_cb), (12 bytes).
    Removing drv_crgu.o(.rev16_text), (4 bytes).
    Removing drv_crgu.o(.revsh_text), (4 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_all_reset_flags), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_reset_flag), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_all_reset_flag), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_reset_flag), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_system_clk), (104 bytes).
    Removing drv_crgu.o(i.drv_crgu_reset_chip), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_clock_src), (16 bytes).
    Removing drv_dma.o(.rev16_text), (4 bytes).
    Removing drv_dma.o(.revsh_text), (4 bytes).
    Removing drv_dma.o(i.drv_dma_apply_handle), (308 bytes).
    Removing drv_dma.o(i.drv_dma_deinit), (52 bytes).
    Removing drv_dma.o(i.drv_dma_disable), (20 bytes).
    Removing drv_dma.o(i.drv_dma_disable_int), (40 bytes).
    Removing drv_dma.o(i.drv_dma_enable), (36 bytes).
    Removing drv_dma.o(i.drv_dma_enable_int), (68 bytes).
    Removing drv_dma.o(i.drv_dma_get_remaining_trans_num), (20 bytes).
    Removing drv_dma.o(i.drv_dma_get_status), (20 bytes).
    Removing drv_dma.o(i.drv_dma_init), (22 bytes).
    Removing drv_dma.o(i.drv_dma_int_list_delete), (88 bytes).
    Removing drv_dma.o(i.drv_dma_int_list_inset), (48 bytes).
    Removing drv_dma.o(i.drv_dma_register_callback), (4 bytes).
    Removing drv_dma.o(i.drv_dma_reset), (36 bytes).
    Removing drv_dma.o(i.drv_dma_set_bitwide), (56 bytes).
    Removing drv_dma.o(i.drv_dma_set_burst), (20 bytes).
    Removing drv_dma.o(i.drv_dma_set_circle_mode), (40 bytes).
    Removing drv_dma.o(i.drv_dma_set_dir), (40 bytes).
    Removing drv_dma.o(i.drv_dma_set_increment), (72 bytes).
    Removing drv_dma.o(i.drv_dma_set_mem_trans_info), (40 bytes).
    Removing drv_dma.o(i.drv_dma_set_mem_trans_offset), (24 bytes).
    Removing drv_dma.o(i.drv_dma_set_per_address), (20 bytes).
    Removing drv_dma.o(i.drv_dma_set_priority), (32 bytes).
    Removing drv_dma.o(i.drv_dma_set_tran_int_cnt), (28 bytes).
    Removing drv_dma.o(i.drv_dma_update_handle_setting), (148 bytes).
    Removing drv_dma.o(i.drv_dma_update_req_by_default), (40 bytes).
    Removing drv_dma.o(.constdata), (136 bytes).
    Removing drv_dsc_dec.o(.rev16_text), (4 bytes).
    Removing drv_dsc_dec.o(.revsh_text), (4 bytes).
    Removing drv_gpio.o(.rev16_text), (4 bytes).
    Removing drv_gpio.o(.revsh_text), (4 bytes).
    Removing drv_gpio.o(i.drv_gpio_get_input_data), (24 bytes).
    Removing drv_pwr.o(.rev16_text), (4 bytes).
    Removing drv_pwr.o(.revsh_text), (4 bytes).
    Removing drv_pwr.o(i.drv_pwr_10bit_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_analog_pwm_en), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_charge_pump_en), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_close_iov18_tp18), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_dsc_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_elvcc_pwm_en), (124 bytes).
    Removing drv_pwr.o(i.drv_pwr_enter_sleep_mode), (152 bytes).
    Removing drv_pwr.o(i.drv_pwr_exit_sleep_mode_ex), (40 bytes).
    Removing drv_pwr.o(i.drv_pwr_fb_pd), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_get_wakeflag), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_get_write_lock_st), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_hf_frm_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_10M_clock), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_mode_clock_sel), (60 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_mode_sel), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_voltage_set), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo11d_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo13s_en), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo13s_set), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo15_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo18s_en), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo18s_set), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_ltpo_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_osc32k_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_osc80m_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_p3k_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_por_mode_flag), (32 bytes).
    Removing drv_pwr.o(i.drv_pwr_power_in), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_power_ready_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_power_sel), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwm_output_pwm_led), (56 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_driver_current_Big_step), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_driver_current_small_step), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_electric_current), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_open_drain), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_ram_pd_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_read_boot_chipst), (12 bytes).
    Removing drv_pwr.o(i.drv_pwr_read_chipcfg), (12 bytes).
    Removing drv_pwr.o(i.drv_pwr_rgbr_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_ap_rst_mode), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_ldo11_mode), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_ldo15_mode), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_pvd_mode), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_system_clk), (32 bytes).
    Removing drv_pwr.o(i.drv_pwr_sw_tp18_en), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_wakeflag_get), (16 bytes).
    Removing drv_spi_master.o(.rev16_text), (4 bytes).
    Removing drv_spi_master.o(.revsh_text), (4 bytes).
    Removing drv_spi_master.o(i.drv_spim_disable), (16 bytes).
    Removing drv_spi_master.o(i.drv_spim_disable_dma_req), (16 bytes).
    Removing drv_spi_master.o(i.drv_spim_enable), (16 bytes).
    Removing drv_spi_master.o(i.drv_spim_enable_dma_req), (16 bytes).
    Removing drv_spi_master.o(i.drv_spim_enable_int), (40 bytes).
    Removing drv_spi_master.o(i.drv_spim_flush), (16 bytes).
    Removing drv_spi_master.o(i.drv_spim_init), (104 bytes).
    Removing drv_spi_master.o(i.drv_spim_read), (100 bytes).
    Removing drv_spi_master.o(i.drv_spim_register_callback), (12 bytes).
    Removing drv_spi_master.o(i.drv_spim_write), (56 bytes).
    Removing drv_spi_master.o(.data), (4 bytes).
    Removing drv_swire.o(.rev16_text), (4 bytes).
    Removing drv_swire.o(.revsh_text), (4 bytes).
    Removing drv_sys_cfg.o(.rev16_text), (4 bytes).
    Removing drv_sys_cfg.o(.revsh_text), (4 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_calib_systick), (12 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_clear_spid_int), (16 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_enable_rx_hs_test), (28 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_enter_lp_mode), (24 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_force_sleep), (28 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_read_spid_int), (16 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_read_version0_id), (12 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_sel_dma_req), (128 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_sel_td_rst_trig), (36 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_set_ap_reset), (28 bytes).
    Removing drv_timer.o(.rev16_text), (4 bytes).
    Removing drv_timer.o(.revsh_text), (4 bytes).
    Removing drv_timer.o(i.drv_timer_get_status), (38 bytes).
    Removing drv_wdg.o(.rev16_text), (4 bytes).
    Removing drv_wdg.o(.revsh_text), (4 bytes).
    Removing drv_wdg.o(i.drv_wdg_enable), (32 bytes).
    Removing drv_wdg.o(i.drv_wdg_load_match), (12 bytes).
    Removing drv_wdg.o(i.drv_wdg_register_callback), (12 bytes).
    Removing drv_wdg.o(i.drv_wdg_sel_mode), (28 bytes).
    Removing drv_wdg.o(i.drv_wdg_set_repeat), (12 bytes).
    Removing drv_crc.o(.rev16_text), (4 bytes).
    Removing drv_crc.o(.revsh_text), (4 bytes).
    Removing drv_crc.o(i.drv_crc_dma_disable), (16 bytes).
    Removing drv_crc.o(i.drv_crc_dma_enable), (16 bytes).
    Removing drv_crc.o(i.drv_crc_get_data_register), (12 bytes).
    Removing drv_crc.o(i.drv_crc_get_fxor_register), (16 bytes).
    Removing drv_crc.o(i.drv_crc_get_idr_counter), (12 bytes).
    Removing drv_crc.o(i.drv_crc_get_initial_seed_register), (12 bytes).
    Removing drv_crc.o(i.drv_crc_get_polynomial_register), (12 bytes).
    Removing drv_crc.o(i.drv_crc_get_rev_in_register), (16 bytes).
    Removing drv_crc.o(i.drv_crc_get_rev_out_register), (16 bytes).
    Removing drv_crc.o(i.drv_crc_get_tcrc_register), (16 bytes).
    Removing drv_crc.o(i.drv_crc_reset), (16 bytes).
    Removing drv_crc.o(i.drv_crc_set_fxor_register), (28 bytes).
    Removing drv_crc.o(i.drv_crc_set_initial_seed_register), (12 bytes).
    Removing drv_crc.o(i.drv_crc_set_polynomial_register), (12 bytes).
    Removing drv_crc.o(i.drv_crc_set_rev_in_register), (24 bytes).
    Removing drv_crc.o(i.drv_crc_set_rev_out_register), (28 bytes).
    Removing drv_crc.o(i.drv_crc_set_tcrc_register), (28 bytes).
    Removing drv_crc.o(i.drv_crc_write_data_register), (28 bytes).
    Removing drv_i2c.o(.rev16_text), (4 bytes).
    Removing drv_i2c.o(.revsh_text), (4 bytes).
    Removing drv_i2c.o(i.__NVIC_DisableIRQ), (32 bytes).
    Removing drv_i2c.o(i.drv_i2c_NVIC_enable), (52 bytes).
    Removing drv_i2c.o(i.drv_i2c_clear_intr_status), (68 bytes).
    Removing drv_i2c.o(i.drv_i2c_clock_enable), (52 bytes).
    Removing drv_i2c.o(i.drv_i2c_disable_dma_req), (24 bytes).
    Removing drv_i2c.o(i.drv_i2c_disable_intr), (20 bytes).
    Removing drv_i2c.o(i.drv_i2c_enable), (36 bytes).
    Removing drv_i2c.o(i.drv_i2c_enable_dma_req), (24 bytes).
    Removing drv_i2c.o(i.drv_i2c_enable_intr), (56 bytes).
    Removing drv_i2c.o(i.drv_i2c_flush), (24 bytes).
    Removing drv_i2c.o(i.drv_i2c_get_fifo_status), (36 bytes).
    Removing drv_i2c.o(i.drv_i2c_get_intr_status), (16 bytes).
    Removing drv_i2c.o(i.drv_i2c_get_rx_count), (20 bytes).
    Removing drv_i2c.o(i.drv_i2c_get_tx_abrtsource), (20 bytes).
    Removing drv_i2c.o(i.drv_i2c_read_data), (44 bytes).
    Removing drv_i2c.o(i.drv_i2c_set_callback), (16 bytes).
    Removing drv_i2c.o(i.drv_i2c_set_fifo_threshold), (32 bytes).
    Removing drv_i2c.o(i.drv_i2c_set_sys_mask), (48 bytes).
    Removing drv_i2c.o(i.drv_i2c_write_data), (40 bytes).
    Removing drv_i2c.o(i.drv_i2cm_cal_scl_cnt), (40 bytes).
    Removing drv_i2c.o(i.drv_i2cm_init), (148 bytes).
    Removing drv_i2c.o(i.drv_i2cm_read_data), (140 bytes).
    Removing drv_i2c.o(i.drv_i2cm_set_baud_rate), (72 bytes).
    Removing drv_i2c.o(i.drv_i2cm_set_slave_addr), (52 bytes).
    Removing drv_i2c.o(i.drv_i2cm_write_data), (76 bytes).
    Removing drv_i2c.o(i.drv_i2cm_write_read_cmd), (60 bytes).
    Removing drv_i2c.o(i.drv_i2cs_init), (72 bytes).
    Removing drv_i2c.o(i.drv_i2cs_own_addr), (16 bytes).
    Removing dcs_packet_fifo.o(.rev16_text), (4 bytes).
    Removing dcs_packet_fifo.o(.revsh_text), (4 bytes).
    Removing dcs_packet_fifo.o(i.dcs_packet_get_fifo_size), (16 bytes).
    Removing drv_se.o(.rev16_text), (4 bytes).
    Removing drv_se.o(.revsh_text), (4 bytes).
    Removing drv_dsi_rx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_rx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_force_video_crtl), (28 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_lpdt_fifo_status), (16 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size), (12 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate), (68 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_version), (12 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg), (24 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_drv_log_level), (12 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg), (48 bytes).
    Removing drv_dsi_tx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_tx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_force_interrupt), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_get_phy_status), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_forcepll), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_start), (24 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot), (68 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger), (92 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter), (296 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit), (228 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_sdf_3d), (32 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_bta), (28 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_vpg), (100 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_version), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_vid_shadow), (20 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_clear), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_lock), (32 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_read), (16 bytes).
    Removing drv_lcdc.o(.rev16_text), (4 bytes).
    Removing drv_lcdc.o(.revsh_text), (4 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_clear_irq), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_dpisignal_output_ctrl), (44 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_fixed_frame_output), (56 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_dpbuf_num), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_dpi_status), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_frame_clk_count), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_int_en_status), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_int_status), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_line_status), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_rgb2pen_subpixel), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_part_display_config), (52 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_pixel_value_config), (32 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_rd_st_line_config), (28 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_software_reset), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_update_shadow_reg), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_vid_sw_start), (56 bytes).
    Removing drv_memc.o(.rev16_text), (4 bytes).
    Removing drv_memc.o(.revsh_text), (4 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_frm_time), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_int_frame), (36 bytes).
    Removing drv_memc.o(i.drv_memc_set_double_buffer_reverse), (24 bytes).
    Removing drv_memc.o(i.drv_memc_set_fb_pri), (44 bytes).
    Removing drv_memc.o(i.drv_memc_set_fb_remaining_line_trigger), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_inten), (28 bytes).
    Removing drv_memc.o(i.drv_memc_set_read_trigger_line), (24 bytes).
    Removing drv_memc.o(i.drv_memc_set_te_ind), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_tear_hwclr), (24 bytes).
    Removing drv_memc.o(i.drv_memc_set_vidc_fb_arb), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_write_trigger_line), (24 bytes).
    Removing drv_rxbr.o(.rev16_text), (4 bytes).
    Removing drv_rxbr.o(.revsh_text), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_clr_swp_cnt), (16 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_dsc_flush), (24 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_col_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_cur_hline_rcv_cnt), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_frame_data_interval), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_hline_dcat), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_ipi_vsync_interval), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_page_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_pix_fmt), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_swpxl_cnt), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg), (20 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_register_irq0_callback), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header), (24 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_ack_pkt_md), (28 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_cmd_filter), (320 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_col_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_compress), (32 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_data_catch_hline), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_page_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_swpxl_data), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_tmpdith_bp), (28 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_soft_reset), (32 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_swpxl_clr), (32 bytes).
    Removing drv_vidc.o(.rev16_text), (4 bytes).
    Removing drv_vidc.o(.revsh_text), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_clear_status0), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_cap_pixel), (28 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_signal_frame), (36 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status0), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status1), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status2), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_dsc_thresh), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_frmst_latency), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_inff_thresh), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_irq_line), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_module_enable), (28 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_outff_thresh), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_update_src_format), (20 bytes).
    Removing drv_uart.o(.rev16_text), (4 bytes).
    Removing drv_uart.o(.revsh_text), (4 bytes).
    Removing drv_uart.o(i.drv_uart_deinit), (60 bytes).
    Removing drv_uart.o(i.drv_uart_get_def_cfg), (72 bytes).
    Removing drv_uart.o(i.drv_uart_recv_blocking), (48 bytes).
    Removing drv_uart.o(i.drv_uart_recv_none_blocking), (60 bytes).
    Removing drv_uart.o(i.drv_uart_send_none_blocking), (60 bytes).
    Removing drv_efuse.o(.rev16_text), (4 bytes).
    Removing drv_efuse.o(.revsh_text), (4 bytes).
    Removing drv_efuse.o(i.drv_efuse_crc_cal), (128 bytes).
    Removing drv_efuse.o(i.drv_efuse_get_default_config), (26 bytes).
    Removing drv_efuse.o(i.drv_efuse_int_disable), (12 bytes).
    Removing drv_efuse.o(i.drv_efuse_write), (56 bytes).
    Removing drv_efuse.o(i.drv_efuse_write_read_req_clear), (22 bytes).
    Removing drv_efuse.o(i.drv_efuse_write_req), (22 bytes).
    Removing drv_phy_common.o(.rev16_text), (4 bytes).
    Removing drv_phy_common.o(.revsh_text), (4 bytes).

560 unused section(s) (total 29041 bytes) removed from the image.

==============================================================================

Image Symbol Table

    Local Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    ../clib/../cmprslib/zerorunl2.c          0x00000000   Number         0  __dczerorl2.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uldiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  idiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uidiv.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry5.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry2.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10b.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llsshr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llushr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llshl.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf7.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf3.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf8.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf2.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfa.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfb.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf1.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf0.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf6.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf5.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf4.o ABSOLUTE
    ../clib/microlib/printf/stubs.s          0x00000000   Number         0  stubs.o ABSOLUTE
    ../clib/microlib/stdio/streams.c         0x00000000   Number         0  stdout.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpya.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpyb.o ABSOLUTE
    ../clib/microlib/string/memset.c         0x00000000   Number         0  memseta.o ABSOLUTE
    ../clib/microlib/string/strlen.c         0x00000000   Number         0  strlen.o ABSOLUTE
    ../clib/microlib/stubs.s                 0x00000000   Number         0  iusefp.o ABSOLUTE
    ../fplib/microlib/d2f.c                  0x00000000   Number         0  d2f.o ABSOLUTE
    ../fplib/microlib/f2d.c                  0x00000000   Number         0  f2d.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  fadd.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  dadd.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  fdiv.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  ddiv.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  fepilogue.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  depilogue.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixul.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixui.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  ffixui.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  ffltui.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  dfltui.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  dmul.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  fmul.o ABSOLUTE
    ../fplib/microlib/fpscalb.c              0x00000000   Number         0  fscalb.o ABSOLUTE
    ../mathlib/ceil.c                        0x00000000   Number         0  ceil.o ABSOLUTE
    ..\..\..\src\common\tau_delay.c          0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\..\..\src\common\tau_log.c            0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_crc.c 0x00000000   Number         0  drv_crc.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_i2c.c 0x00000000   Number         0  drv_i2c.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_spi_master.c 0x00000000   Number         0  drv_spi_master.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_wdg.c 0x00000000   Number         0  drv_wdg.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_crc.c 0x00000000   Number         0  hal_crc.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_i2c_slave.c 0x00000000   Number         0  hal_i2c_slave.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_pwr.c 0x00000000   Number         0  hal_pwr.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_spi_master.c 0x00000000   Number         0  hal_spi_master.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_swire.c 0x00000000   Number         0  hal_swire.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_timer.c 0x00000000   Number         0  hal_timer.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_wdg.c 0x00000000   Number         0  hal_wdg.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\dcs_packet_fifo.c 0x00000000   Number         0  dcs_packet_fifo.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_dcs.c 0x00000000   Number         0  hal_internal_dcs.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_fb.c 0x00000000   Number         0  hal_internal_fb.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_svs.c 0x00000000   Number         0  hal_internal_svs.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\src\drv_se.c  0x00000000   Number         0  drv_se.o ABSOLUTE
    ..\..\src\app\S8\app_tp_for_custom_s8.c  0x00000000   Number         0  app_tp_for_custom_s8.o ABSOLUTE
    ..\..\src\app\S8\s8_demo.c               0x00000000   Number         0  s8_demo.o ABSOLUTE
    ..\..\src\app\main.c                     0x00000000   Number         0  main.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_crc.c 0x00000000   Number         0  demo_hal_crc.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_dsi_rx.c 0x00000000   Number         0  demo_hal_dsi_rx.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_dsi_tx.c 0x00000000   Number         0  demo_hal_dsi_tx.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_flash.c 0x00000000   Number         0  demo_hal_flash.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_gpio.c 0x00000000   Number         0  demo_hal_gpio.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_i2c.c 0x00000000   Number         0  demo_hal_i2c.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_pwm.c 0x00000000   Number         0  demo_hal_pwm.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_pwr.c 0x00000000   Number         0  demo_hal_pwr.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_spi.c 0x00000000   Number         0  demo_hal_spi.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_swire.c 0x00000000   Number         0  demo_hal_swire.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_uart.c 0x00000000   Number         0  demo_hal_uart.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_wdg.c 0x00000000   Number         0  demo_hal_wdg.o ABSOLUTE
    ..\..\src\app\module_demo\module_demo_main.c 0x00000000   Number         0  module_demo_main.o ABSOLUTE
    ..\..\src\app\touch\app_tp_transfer.c    0x00000000   Number         0  app_tp_transfer.o ABSOLUTE
    ..\..\src\board\board.c                  0x00000000   Number         0  board.o ABSOLUTE
    ..\..\src\board\startup\startup_ARMCM0.s 0x00000000   Number         0  startup_armcm0.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_delay.c     0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_log.c       0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_crc.c 0x00000000   Number         0  drv_crc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_i2c.c 0x00000000   Number         0  drv_i2c.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_spi_master.c 0x00000000   Number         0  drv_spi_master.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_wdg.c 0x00000000   Number         0  drv_wdg.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_crc.c 0x00000000   Number         0  hal_crc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_i2c_slave.c 0x00000000   Number         0  hal_i2c_slave.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_pwr.c 0x00000000   Number         0  hal_pwr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_spi_master.c 0x00000000   Number         0  hal_spi_master.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_swire.c 0x00000000   Number         0  hal_swire.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_timer.c 0x00000000   Number         0  hal_timer.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_wdg.c 0x00000000   Number         0  hal_wdg.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\dcs_packet_fifo.c 0x00000000   Number         0  dcs_packet_fifo.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_dcs.c 0x00000000   Number         0  hal_internal_dcs.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_fb.c 0x00000000   Number         0  hal_internal_fb.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_svs.c 0x00000000   Number         0  hal_internal_svs.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\src\\drv_se.c 0x00000000   Number         0  drv_se.o ABSOLUTE
    ..\\..\\src\\app\\S8\\app_tp_for_custom_s8.c 0x00000000   Number         0  app_tp_for_custom_s8.o ABSOLUTE
    ..\\..\\src\\app\\S8\\s8_demo.c          0x00000000   Number         0  s8_demo.o ABSOLUTE
    ..\\..\\src\\app\\main.c                 0x00000000   Number         0  main.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_crc.c 0x00000000   Number         0  demo_hal_crc.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_dsi_rx.c 0x00000000   Number         0  demo_hal_dsi_rx.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_dsi_tx.c 0x00000000   Number         0  demo_hal_dsi_tx.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_flash.c 0x00000000   Number         0  demo_hal_flash.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_gpio.c 0x00000000   Number         0  demo_hal_gpio.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_i2c.c 0x00000000   Number         0  demo_hal_i2c.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_pwm.c 0x00000000   Number         0  demo_hal_pwm.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_pwr.c 0x00000000   Number         0  demo_hal_pwr.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_spi.c 0x00000000   Number         0  demo_hal_spi.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_swire.c 0x00000000   Number         0  demo_hal_swire.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_uart.c 0x00000000   Number         0  demo_hal_uart.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_wdg.c 0x00000000   Number         0  demo_hal_wdg.o ABSOLUTE
    ..\\..\\src\\app\\touch\\app_tp_transfer.c 0x00000000   Number         0  app_tp_transfer.o ABSOLUTE
    ..\\..\\src\\board\\board.c              0x00000000   Number         0  board.o ABSOLUTE
    cdrcmple.s                               0x00000000   Number         0  cdrcmple.o ABSOLUTE
    cfcmple.s                                0x00000000   Number         0  cfcmple.o ABSOLUTE
    cfrcmple.s                               0x00000000   Number         0  cfrcmple.o ABSOLUTE
    dc.s                                     0x00000000   Number         0  dc.o ABSOLUTE
    handlers.s                               0x00000000   Number         0  handlers.o ABSOLUTE
    init.s                                   0x00000000   Number         0  init.o ABSOLUTE
    RESET                                    0x00010000   Section      192  startup_armcm0.o(RESET)
    .ARM.Collect$$$$00000000                 0x000100c0   Section        0  entry.o(.ARM.Collect$$$$00000000)
    .ARM.Collect$$$$00000001                 0x000100c0   Section        4  entry2.o(.ARM.Collect$$$$00000001)
    .ARM.Collect$$$$00000004                 0x000100c4   Section        4  entry5.o(.ARM.Collect$$$$00000004)
    .ARM.Collect$$$$00000008                 0x000100c8   Section        0  entry7b.o(.ARM.Collect$$$$00000008)
    .ARM.Collect$$$$0000000A                 0x000100c8   Section        0  entry8b.o(.ARM.Collect$$$$0000000A)
    .ARM.Collect$$$$0000000B                 0x000100c8   Section        8  entry9a.o(.ARM.Collect$$$$0000000B)
    .ARM.Collect$$$$0000000D                 0x000100d0   Section        0  entry10a.o(.ARM.Collect$$$$0000000D)
    .ARM.Collect$$$$0000000F                 0x000100d0   Section        0  entry11a.o(.ARM.Collect$$$$0000000F)
    .ARM.Collect$$$$00002712                 0x000100d0   Section        4  entry2.o(.ARM.Collect$$$$00002712)
    __lit__00000000                          0x000100d0   Data           4  entry2.o(.ARM.Collect$$$$00002712)
    .text                                    0x000100d4   Section      120  startup_armcm0.o(.text)
    .text                                    0x0001014c   Section        0  uidiv.o(.text)
    .text                                    0x00010178   Section        0  idiv.o(.text)
    .text                                    0x000101a0   Section        0  memcpya.o(.text)
    .text                                    0x000101c4   Section        0  memseta.o(.text)
    .text                                    0x000101e8   Section        0  strlen.o(.text)
    .text                                    0x000101f6   Section        0  fadd.o(.text)
    .text                                    0x000102a8   Section        0  fmul.o(.text)
    .text                                    0x00010322   Section        0  fdiv.o(.text)
    .text                                    0x0001039e   Section        0  fscalb.o(.text)
    .text                                    0x000103b8   Section        0  dadd.o(.text)
    .text                                    0x0001051c   Section        0  dmul.o(.text)
    .text                                    0x000105ec   Section        0  ddiv.o(.text)
    .text                                    0x000106dc   Section        0  ffltui.o(.text)
    .text                                    0x000106ec   Section        0  dfltui.o(.text)
    .text                                    0x00010708   Section        0  ffixui.o(.text)
    .text                                    0x00010730   Section        0  dfixui.o(.text)
    .text                                    0x0001076c   Section        0  f2d.o(.text)
    .text                                    0x00010794   Section        0  d2f.o(.text)
    .text                                    0x000107cc   Section       20  cfcmple.o(.text)
    .text                                    0x000107e0   Section       20  cfrcmple.o(.text)
    .text                                    0x000107f4   Section        0  uldiv.o(.text)
    .text                                    0x00010854   Section        0  llshl.o(.text)
    .text                                    0x00010874   Section        0  llushr.o(.text)
    .text                                    0x00010896   Section        0  llsshr.o(.text)
    .text                                    0x000108bc   Section        0  iusefp.o(.text)
    .text                                    0x000108bc   Section        0  fepilogue.o(.text)
    .text                                    0x0001093e   Section        0  depilogue.o(.text)
    .text                                    0x000109fc   Section        0  dfixul.o(.text)
    .text                                    0x00010a3c   Section       40  cdrcmple.o(.text)
    .text                                    0x00010a64   Section       36  init.o(.text)
    .text                                    0x00010a88   Section        0  __dczerorl2.o(.text)
    i.AP_NRESET_IRQn_Handler                 0x00010ae0   Section        0  drv_gpio.o(i.AP_NRESET_IRQn_Handler)
    i.DMA_IRQn_Handler                       0x00010afc   Section        0  drv_dma.o(i.DMA_IRQn_Handler)
    i.EXTI_INT0_IRQn_Handler                 0x00010b58   Section        0  drv_gpio.o(i.EXTI_INT0_IRQn_Handler)
    i.EXTI_INT1_IRQn_Handler                 0x00010b62   Section        0  drv_gpio.o(i.EXTI_INT1_IRQn_Handler)
    i.EXTI_INT2_IRQn_Handler                 0x00010b6c   Section        0  drv_gpio.o(i.EXTI_INT2_IRQn_Handler)
    i.EXTI_INT3_IRQn_Handler                 0x00010b76   Section        0  drv_gpio.o(i.EXTI_INT3_IRQn_Handler)
    i.EXTI_INT4_IRQn_Handler                 0x00010b80   Section        0  drv_gpio.o(i.EXTI_INT4_IRQn_Handler)
    i.EXTI_INT5_IRQn_Handler                 0x00010b8a   Section        0  drv_gpio.o(i.EXTI_INT5_IRQn_Handler)
    i.EXTI_INT6_IRQn_Handler                 0x00010b94   Section        0  drv_gpio.o(i.EXTI_INT6_IRQn_Handler)
    i.EXTI_INT7_IRQn_Handler                 0x00010b9e   Section        0  drv_gpio.o(i.EXTI_INT7_IRQn_Handler)
    i.HardFault_Handler                      0x00010ba8   Section        0  drv_common.o(i.HardFault_Handler)
    i.I2C0_IRQn_Handler                      0x00010bf0   Section        0  drv_i2c.o(i.I2C0_IRQn_Handler)
    i.I2C1_IRQn_Handler                      0x00010bfc   Section        0  drv_i2c.o(i.I2C1_IRQn_Handler)
    i.I2C2_IRQn_Handler                      0x00010c08   Section        0  drv_i2c.o(i.I2C2_IRQn_Handler)
    i.LCDC_IRQn_Handler                      0x00010c14   Section        0  hal_internal_vsync.o(i.LCDC_IRQn_Handler)
    i.MEMC_IRQn_Handler                      0x00010cfc   Section        0  drv_memc.o(i.MEMC_IRQn_Handler)
    i.MIPI_TX_IRQn_Handler                   0x00010d98   Section        0  drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler)
    i.SPIM_IRQn_Handler                      0x00010e50   Section        0  hal_spi_master.o(i.SPIM_IRQn_Handler)
    i.SWIRE_IRQn_Handler                     0x00010e90   Section        0  drv_swire.o(i.SWIRE_IRQn_Handler)
    i.SysTick_Handler                        0x00010ec0   Section        0  drv_common.o(i.SysTick_Handler)
    i.TIMER0_IRQn_Handler                    0x00010ed8   Section        0  drv_timer.o(i.TIMER0_IRQn_Handler)
    i.TIMER1_IRQn_Handler                    0x00010ee2   Section        0  drv_timer.o(i.TIMER1_IRQn_Handler)
    i.TIMER2_IRQn_Handler                    0x00010eec   Section        0  drv_timer.o(i.TIMER2_IRQn_Handler)
    i.TIMER3_IRQn_Handler                    0x00010ef6   Section        0  drv_timer.o(i.TIMER3_IRQn_Handler)
    i.VIDC_IRQn_Handler                      0x00010f00   Section        0  drv_vidc.o(i.VIDC_IRQn_Handler)
    i.VPRE1_IRQn_Handler                     0x00010f1c   Section        0  drv_rxbr.o(i.VPRE1_IRQn_Handler)
    i.VPRE_IRQn_Handler                      0x00010f38   Section        0  hal_internal_dcs.o(i.VPRE_IRQn_Handler)
    i.WDG_IRQn_Handler                       0x00010fa4   Section        0  drv_wdg.o(i.WDG_IRQn_Handler)
    i.__0printf                              0x00010fdc   Section        0  printfa.o(i.__0printf)
    i.__scatterload_null                     0x00010ffc   Section        2  handlers.o(i.__scatterload_null)
    .ARM.__at_0x11000                        0x00011000   Section       28  drv_common.o(.ARM.__at_0x11000)
    .ARM.__at_0x1101C                        0x0001101c   Section       16  tau_log.o(.ARM.__at_0x1101C)
    .ARM.__at_0x1102C                        0x0001102c   Section       22  hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C)
    i.MIPI_RX_IRQn_Handler                   0x00011044   Section        0  drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler)
    i.UART_IRQn_Handler                      0x000113a8   Section        0  drv_uart.o(i.UART_IRQn_Handler)
    i.__0vsprintf                            0x00011528   Section        0  printfa.o(i.__0vsprintf)
    i.__ARM_clz                              0x0001154c   Section        0  depilogue.o(i.__ARM_clz)
    i.__ARM_common_switch8                   0x0001157a   Section        0  hal_dsi_rx_ctrl.o(i.__ARM_common_switch8)
    i.__NVIC_DisableIRQ                      0x00011594   Section        0  drv_rxbr.o(i.__NVIC_DisableIRQ)
    __NVIC_DisableIRQ                        0x00011595   Thumb Code    26  drv_rxbr.o(i.__NVIC_DisableIRQ)
    i.__NVIC_EnableIRQ                       0x000115b4   Section        0  drv_rxbr.o(i.__NVIC_EnableIRQ)
    __NVIC_EnableIRQ                         0x000115b5   Thumb Code    18  drv_rxbr.o(i.__NVIC_EnableIRQ)
    i.__scatterload_copy                     0x000115cc   Section       14  handlers.o(i.__scatterload_copy)
    i.__scatterload_zeroinit                 0x000115da   Section       14  handlers.o(i.__scatterload_zeroinit)
    i._fp_digits                             0x000115e8   Section        0  printfa.o(i._fp_digits)
    _fp_digits                               0x000115e9   Thumb Code   344  printfa.o(i._fp_digits)
    i._printf_core                           0x0001175c   Section        0  printfa.o(i._printf_core)
    _printf_core                             0x0001175d   Thumb Code  1754  printfa.o(i._printf_core)
    i._printf_post_padding                   0x00011e48   Section        0  printfa.o(i._printf_post_padding)
    _printf_post_padding                     0x00011e49   Thumb Code    32  printfa.o(i._printf_post_padding)
    i._printf_pre_padding                    0x00011e68   Section        0  printfa.o(i._printf_pre_padding)
    _printf_pre_padding                      0x00011e69   Thumb Code    44  printfa.o(i._printf_pre_padding)
    i._sputc                                 0x00011e94   Section        0  printfa.o(i._sputc)
    _sputc                                   0x00011e95   Thumb Code    10  printfa.o(i._sputc)
    i.ap_dcs_set_backlight                   0x00011ea0   Section        0  s8_demo.o(i.ap_dcs_set_backlight)
    ap_dcs_set_backlight                     0x00011ea1   Thumb Code   158  s8_demo.o(i.ap_dcs_set_backlight)
    i.ap_dcs_set_display_off                 0x00011f50   Section        0  s8_demo.o(i.ap_dcs_set_display_off)
    ap_dcs_set_display_off                   0x00011f51   Thumb Code    34  s8_demo.o(i.ap_dcs_set_display_off)
    i.ap_dcs_set_display_on                  0x00011f9c   Section        0  s8_demo.o(i.ap_dcs_set_display_on)
    ap_dcs_set_display_on                    0x00011f9d   Thumb Code    28  s8_demo.o(i.ap_dcs_set_display_on)
    i.ap_dcs_set_enter_sleep_mode            0x00011fd8   Section        0  s8_demo.o(i.ap_dcs_set_enter_sleep_mode)
    ap_dcs_set_enter_sleep_mode              0x00011fd9   Thumb Code    92  s8_demo.o(i.ap_dcs_set_enter_sleep_mode)
    i.ap_dcs_set_exit_sleep_mode             0x00012060   Section        0  s8_demo.o(i.ap_dcs_set_exit_sleep_mode)
    ap_dcs_set_exit_sleep_mode               0x00012061   Thumb Code    50  s8_demo.o(i.ap_dcs_set_exit_sleep_mode)
    i.ap_rstn_pull_high_cb                   0x000120c4   Section        0  s8_demo.o(i.ap_rstn_pull_high_cb)
    ap_rstn_pull_high_cb                     0x000120c5   Thumb Code    22  s8_demo.o(i.ap_rstn_pull_high_cb)
    i.ap_set_framerate                       0x000120e0   Section        0  s8_demo.o(i.ap_set_framerate)
    ap_set_framerate                         0x000120e1   Thumb Code    44  s8_demo.o(i.ap_set_framerate)
    i.ap_update_pps_9E                       0x00012134   Section        0  s8_demo.o(i.ap_update_pps_9E)
    ap_update_pps_9E                         0x00012135   Thumb Code   122  s8_demo.o(i.ap_update_pps_9E)
    i.app_display_init                       0x000121b8   Section        0  s8_demo.o(i.app_display_init)
    i.app_gpio_init                          0x00012220   Section        0  s8_demo.o(i.app_gpio_init)
    i.app_init_panel                         0x00012240   Section        0  s8_demo.o(i.app_init_panel)
    app_init_panel                           0x00012241   Thumb Code    64  s8_demo.o(i.app_init_panel)
    i.app_mipi_rx_init                       0x00012288   Section        0  s8_demo.o(i.app_mipi_rx_init)
    app_mipi_rx_init                         0x00012289   Thumb Code   212  s8_demo.o(i.app_mipi_rx_init)
    i.app_mipi_tx_init                       0x00012370   Section        0  s8_demo.o(i.app_mipi_tx_init)
    app_mipi_tx_init                         0x00012371   Thumb Code   188  s8_demo.o(i.app_mipi_tx_init)
    i.app_mipi_tx_start                      0x00012430   Section        0  s8_demo.o(i.app_mipi_tx_start)
    app_mipi_tx_start                        0x00012431   Thumb Code    62  s8_demo.o(i.app_mipi_tx_start)
    i.app_set_dcs_hw_ack                     0x0001249c   Section        0  s8_demo.o(i.app_set_dcs_hw_ack)
    app_set_dcs_hw_ack                       0x0001249d   Thumb Code   134  s8_demo.o(i.app_set_dcs_hw_ack)
    i.app_system_process                     0x00012528   Section        0  s8_demo.o(i.app_system_process)
    app_system_process                       0x00012529   Thumb Code    62  s8_demo.o(i.app_system_process)
    i.app_system_resume                      0x00012574   Section        0  s8_demo.o(i.app_system_resume)
    app_system_resume                        0x00012575   Thumb Code    30  s8_demo.o(i.app_system_resume)
    i.app_system_suspend                     0x000125bc   Section        0  s8_demo.o(i.app_system_suspend)
    app_system_suspend                       0x000125bd   Thumb Code   150  s8_demo.o(i.app_system_suspend)
    i.app_tx_panel_reset                     0x000126b0   Section        0  s8_demo.o(i.app_tx_panel_reset)
    app_tx_panel_reset                       0x000126b1   Thumb Code    46  s8_demo.o(i.app_tx_panel_reset)
    i.board_Init                             0x000126e0   Section        0  board.o(i.board_Init)
    i.ceil                                   0x0001270c   Section        0  ceil.o(i.ceil)
    i.check_mipi_rx_tx_video_info            0x000127d4   Section        0  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    check_mipi_rx_tx_video_info              0x000127d5   Thumb Code    44  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    i.check_pkt_buf_rev                      0x00012800   Section        0  hal_internal_dcs.o(i.check_pkt_buf_rev)
    check_pkt_buf_rev                        0x00012801   Thumb Code    84  hal_internal_dcs.o(i.check_pkt_buf_rev)
    i.dcs_packet_fifo_alloc                  0x00012888   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    i.dcs_packet_fifo_init                   0x000128e0   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    i.dcs_packet_free_fifo_header            0x000128f8   Section        0  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    i.dcs_packet_get_fifo_header             0x0001293c   Section        0  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    i.delayMs                                0x00012960   Section        0  tau_delay.o(i.delayMs)
    i.delayUs                                0x00012978   Section        0  tau_delay.o(i.delayUs)
    i.drv_common_system_init                 0x000129a4   Section        0  drv_common.o(i.drv_common_system_init)
    i.drv_crgu_enable_clock                  0x000129ac   Section        0  drv_crgu.o(i.drv_crgu_enable_clock)
    i.drv_crgu_get_rxbr_clk                  0x000129e8   Section        0  drv_crgu.o(i.drv_crgu_get_rxbr_clk)
    i.drv_crgu_reset_modules                 0x00012a50   Section        0  drv_crgu.o(i.drv_crgu_reset_modules)
    i.drv_crgu_set_ahb_clk                   0x00012a60   Section        0  drv_crgu.o(i.drv_crgu_set_ahb_clk)
    i.drv_crgu_set_clock_div                 0x00012a88   Section        0  drv_crgu.o(i.drv_crgu_set_clock_div)
    i.drv_crgu_set_dpi_clk                   0x00012a98   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_clk)
    i.drv_crgu_set_dsc_clk                   0x00012ad4   Section        0  drv_crgu.o(i.drv_crgu_set_dsc_clk)
    i.drv_crgu_set_fb_clk                    0x00012b0c   Section        0  drv_crgu.o(i.drv_crgu_set_fb_clk)
    i.drv_crgu_set_lcdc_clk                  0x00012b34   Section        0  drv_crgu.o(i.drv_crgu_set_lcdc_clk)
    i.drv_crgu_set_reset                     0x00012b5c   Section        0  drv_crgu.o(i.drv_crgu_set_reset)
    i.drv_crgu_set_rxbr_clk                  0x00012b74   Section        0  drv_crgu.o(i.drv_crgu_set_rxbr_clk)
    i.drv_crgu_set_vidc_clk                  0x00012b9c   Section        0  drv_crgu.o(i.drv_crgu_set_vidc_clk)
    i.drv_dma_clear_status                   0x00012bc4   Section        0  drv_dma.o(i.drv_dma_clear_status)
    i.drv_dma_get_int_source                 0x00012bdc   Section        0  drv_dma.o(i.drv_dma_get_int_source)
    drv_dma_get_int_source                   0x00012bdd   Thumb Code    16  drv_dma.o(i.drv_dma_get_int_source)
    i.drv_dsc_dec_disable                    0x00012bf0   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    i.drv_dsc_dec_enable                     0x00012c0c   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    i.drv_dsc_dec_get_nslc                   0x00012c48   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    i.drv_dsi_rx_calc_ipi_tx_delay           0x00012c68   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    i.drv_dsi_rx_enable_irq                  0x00012d74   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    i.drv_dsi_rx_get_color_bpp               0x00012db4   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    drv_dsi_rx_get_color_bpp                 0x00012db5   Thumb Code    62  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    i.drv_dsi_rx_get_color_pcc               0x00012e04   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    drv_dsi_rx_get_color_pcc                 0x00012e05   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    i.drv_dsi_rx_get_compression_en          0x00012e20   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    i.drv_dsi_rx_get_ddi_crc_en              0x00012e30   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_ddi_crc_en)
    i.drv_dsi_rx_power_up                    0x00012e40   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    i.drv_dsi_rx_set_check_crc               0x00012e58   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc)
    i.drv_dsi_rx_set_ctrl_cfg                0x00012e74   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    i.drv_dsi_rx_set_ddi_cfg                 0x00012e98   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    i.drv_dsi_rx_set_ddi_crc_en              0x00012ea8   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_crc_en)
    i.drv_dsi_rx_set_inten                   0x00012ec4   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    i.drv_dsi_rx_set_ipi_cfg                 0x00012ed0   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    i.drv_dsi_rx_set_ipi_ycbcr_frmt          0x00012ee0   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_ycbcr_frmt)
    i.drv_dsi_rx_set_lane_swap               0x00012efc   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    i.drv_dsi_rx_set_resp_cnt                0x00012f10   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    i.drv_dsi_rx_set_tear_resp_en            0x00012f34   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_tear_resp_en)
    i.drv_dsi_rx_set_up_phy                  0x00012f50   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    i.drv_dsi_rx_shut_down                   0x00012fe8   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    i.drv_dsi_tx_command_header              0x00013000   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    i.drv_dsi_tx_command_mode_cfg            0x00013018   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    i.drv_dsi_tx_command_put_payload         0x00013070   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    i.drv_dsi_tx_config_eotp                 0x0001307c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    i.drv_dsi_tx_config_int                  0x0001309c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    i.drv_dsi_tx_dpi_lpcmd_time              0x000130a8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    i.drv_dsi_tx_dpi_mode                    0x000130b8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    i.drv_dsi_tx_dpi_polarity                0x000130c8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    i.drv_dsi_tx_edpi_cmd_size               0x000130ec   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    i.drv_dsi_tx_get_cmd_status              0x000130f8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    i.drv_dsi_tx_mode                        0x00013104   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    i.drv_dsi_tx_phy_clock_lane_auto_lp      0x00013110   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    i.drv_dsi_tx_phy_clock_lane_req_hs       0x0001312c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    i.drv_dsi_tx_phy_lane_mode               0x0001314c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    i.drv_dsi_tx_phy_status_ready            0x0001315c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    i.drv_dsi_tx_phy_status_stopstate        0x000131c4   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    i.drv_dsi_tx_phy_test_setup              0x00013208   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    i.drv_dsi_tx_phy_time_cfg                0x00013358   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    i.drv_dsi_tx_powerup                     0x00013378   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    i.drv_dsi_tx_response_mode               0x00013384   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    i.drv_dsi_tx_set_bta_ack                 0x000133a8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    i.drv_dsi_tx_set_esc_div                 0x000133c4   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    i.drv_dsi_tx_set_int                     0x000133d8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    i.drv_dsi_tx_set_time_out_div            0x00013418   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    i.drv_dsi_tx_set_video_chunk             0x00013430   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    i.drv_dsi_tx_set_video_timing            0x00013444   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    i.drv_dsi_tx_shutdown                    0x00013468   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    i.drv_dsi_tx_timeout_cfg                 0x00013474   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    i.drv_dsi_tx_video_mode_cfg              0x000134a0   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    i.drv_efuse_enter_inactive               0x00013588   Section        0  drv_efuse.o(i.drv_efuse_enter_inactive)
    i.drv_efuse_int_enable                   0x000135be   Section        0  drv_efuse.o(i.drv_efuse_int_enable)
    i.drv_efuse_read                         0x000135ca   Section        0  drv_efuse.o(i.drv_efuse_read)
    i.drv_efuse_read_req                     0x00013604   Section        0  drv_efuse.o(i.drv_efuse_read_req)
    i.drv_gpio_get_attribute                 0x0001361c   Section        0  drv_gpio.o(i.drv_gpio_get_attribute)
    i.drv_gpio_handle_int                    0x0001362c   Section        0  drv_gpio.o(i.drv_gpio_handle_int)
    drv_gpio_handle_int                      0x0001362d   Thumb Code    30  drv_gpio.o(i.drv_gpio_handle_int)
    i.drv_gpio_register_ap_reset_callback    0x00013650   Section        0  drv_gpio.o(i.drv_gpio_register_ap_reset_callback)
    i.drv_gpio_register_callback             0x0001365c   Section        0  drv_gpio.o(i.drv_gpio_register_callback)
    i.drv_gpio_set_attribute                 0x00013670   Section        0  drv_gpio.o(i.drv_gpio_set_attribute)
    i.drv_gpio_set_int                       0x0001368c   Section        0  drv_gpio.o(i.drv_gpio_set_int)
    i.drv_gpio_set_ioe                       0x000136d0   Section        0  drv_gpio.o(i.drv_gpio_set_ioe)
    i.drv_gpio_set_mode                      0x000136f0   Section        0  drv_gpio.o(i.drv_gpio_set_mode)
    i.drv_gpio_set_output_data               0x00013704   Section        0  hal_gpio.o(i.drv_gpio_set_output_data)
    drv_gpio_set_output_data                 0x00013705   Thumb Code    26  hal_gpio.o(i.drv_gpio_set_output_data)
    i.drv_lcdc_bcsa_config                   0x00013724   Section        0  drv_lcdc.o(i.drv_lcdc_bcsa_config)
    i.drv_lcdc_cfg_int_frame                 0x0001374c   Section        0  drv_lcdc.o(i.drv_lcdc_cfg_int_frame)
    i.drv_lcdc_clear_int                     0x00013778   Section        0  drv_lcdc.o(i.drv_lcdc_clear_int)
    drv_lcdc_clear_int                       0x00013779   Thumb Code    20  drv_lcdc.o(i.drv_lcdc_clear_int)
    i.drv_lcdc_cmd_start                     0x00013790   Section        0  drv_lcdc.o(i.drv_lcdc_cmd_start)
    i.drv_lcdc_config_acc_command_mode       0x000137c4   Section        0  drv_lcdc.o(i.drv_lcdc_config_acc_command_mode)
    i.drv_lcdc_config_int                    0x000137d8   Section        0  drv_lcdc.o(i.drv_lcdc_config_int)
    i.drv_lcdc_config_int_single             0x00013810   Section        0  drv_lcdc.o(i.drv_lcdc_config_int_single)
    i.drv_lcdc_config_overwrite_rgb          0x00013838   Section        0  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    i.drv_lcdc_config_src_parameter          0x00013850   Section        0  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    i.drv_lcdc_crop_hact                     0x000138a0   Section        0  drv_lcdc.o(i.drv_lcdc_crop_hact)
    i.drv_lcdc_ctrl_flow                     0x000138b0   Section        0  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    i.drv_lcdc_dith_config                   0x000138e8   Section        0  drv_lcdc.o(i.drv_lcdc_dith_config)
    i.drv_lcdc_edge_dect_config              0x00013918   Section        0  drv_lcdc.o(i.drv_lcdc_edge_dect_config)
    i.drv_lcdc_edge_enh_config               0x00013954   Section        0  drv_lcdc.o(i.drv_lcdc_edge_enh_config)
    i.drv_lcdc_enable_shadow_reg             0x000139b8   Section        0  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    i.drv_lcdc_endianness_config             0x000139dc   Section        0  drv_lcdc.o(i.drv_lcdc_endianness_config)
    i.drv_lcdc_fc_config                     0x000139f8   Section        0  drv_lcdc.o(i.drv_lcdc_fc_config)
    i.drv_lcdc_fldc_config                   0x00013a18   Section        0  drv_lcdc.o(i.drv_lcdc_fldc_config)
    i.drv_lcdc_function_disable              0x00013a3c   Section        0  drv_lcdc.o(i.drv_lcdc_function_disable)
    i.drv_lcdc_function_enable               0x00013a60   Section        0  drv_lcdc.o(i.drv_lcdc_function_enable)
    i.drv_lcdc_set_int                       0x00013a84   Section        0  drv_lcdc.o(i.drv_lcdc_set_int)
    i.drv_lcdc_set_prefetch                  0x00013ac0   Section        0  drv_lcdc.o(i.drv_lcdc_set_prefetch)
    i.drv_lcdc_set_tear_line                 0x00013adc   Section        0  drv_lcdc.o(i.drv_lcdc_set_tear_line)
    i.drv_lcdc_stop_display                  0x00013af8   Section        0  drv_lcdc.o(i.drv_lcdc_stop_display)
    i.drv_lcdc_vid_hw_start                  0x00013b08   Section        0  drv_lcdc.o(i.drv_lcdc_vid_hw_start)
    i.drv_lcdc_vintp_mode_config             0x00013b44   Section        0  drv_lcdc.o(i.drv_lcdc_vintp_mode_config)
    i.drv_memc_clear_status                  0x00013b5c   Section        0  drv_memc.o(i.drv_memc_clear_status)
    i.drv_memc_enable_irq                    0x00013b70   Section        0  drv_memc.o(i.drv_memc_enable_irq)
    i.drv_memc_gen_a_tear_signal             0x00013bb0   Section        0  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    i.drv_memc_get_status                    0x00013bc0   Section        0  drv_memc.o(i.drv_memc_get_status)
    i.drv_memc_get_tear_mode                 0x00013bd8   Section        0  drv_memc.o(i.drv_memc_get_tear_mode)
    i.drv_memc_rate_transfer_sel             0x00013be8   Section        0  drv_memc.o(i.drv_memc_rate_transfer_sel)
    i.drv_memc_sel_vsync                     0x00013c04   Section        0  drv_memc.o(i.drv_memc_sel_vsync)
    i.drv_memc_set_active_height             0x00013c18   Section        0  drv_memc.o(i.drv_memc_set_active_height)
    i.drv_memc_set_circ_mode_enable          0x00013c30   Section        0  drv_memc.o(i.drv_memc_set_circ_mode_enable)
    i.drv_memc_set_data_mode                 0x00013c4c   Section        0  drv_memc.o(i.drv_memc_set_data_mode)
    i.drv_memc_set_double_buffer             0x00013c60   Section        0  drv_memc.o(i.drv_memc_set_double_buffer)
    i.drv_memc_set_frame_drop_select         0x00013c78   Section        0  drv_memc.o(i.drv_memc_set_frame_drop_select)
    i.drv_memc_set_fs_en_conditions          0x00013c94   Section        0  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    i.drv_memc_set_lcdc_st_conditions        0x00013cac   Section        0  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    i.drv_memc_set_ltpo_mode                 0x00013cc8   Section        0  drv_memc.o(i.drv_memc_set_ltpo_mode)
    i.drv_memc_set_ltpo_pu_thres             0x00013ce8   Section        0  drv_memc.o(i.drv_memc_set_ltpo_pu_thres)
    i.drv_memc_set_tear_mode                 0x00013d00   Section        0  drv_memc.o(i.drv_memc_set_tear_mode)
    i.drv_memc_set_tear_waveform             0x00013d14   Section        0  drv_memc.o(i.drv_memc_set_tear_waveform)
    i.drv_memc_set_vidc_sync_cnt             0x00013d40   Section        0  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    i.drv_phy_test_clear                     0x00013d54   Section        0  drv_phy_common.o(i.drv_phy_test_clear)
    i.drv_phy_test_lock                      0x00013d64   Section        0  drv_phy_common.o(i.drv_phy_test_lock)
    i.drv_pwr_efuse_pd                       0x00013d7c   Section        0  drv_pwr.o(i.drv_pwr_efuse_pd)
    i.drv_pwr_enter_deep_sleep_mode          0x00013dac   Section        0  drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode)
    i.drv_pwr_enter_sleep_mode_ex            0x00013dec   Section        0  drv_pwr.o(i.drv_pwr_enter_sleep_mode_ex)
    i.drv_pwr_enter_stop_sleep_mode          0x00013e14   Section        0  drv_pwr.o(i.drv_pwr_enter_stop_sleep_mode)
    i.drv_pwr_exit_sleep_mode                0x00013ea0   Section        0  drv_pwr.o(i.drv_pwr_exit_sleep_mode)
    i.drv_pwr_get_power_ready_st             0x00013ec8   Section        0  drv_pwr.o(i.drv_pwr_get_power_ready_st)
    i.drv_pwr_set_breath_screen_power_sel    0x00013ed8   Section        0  drv_pwr.o(i.drv_pwr_set_breath_screen_power_sel)
    i.drv_pwr_set_digit_power_sel            0x00013f00   Section        0  drv_pwr.o(i.drv_pwr_set_digit_power_sel)
    i.drv_pwr_set_pll_clk                    0x00013f28   Section        0  drv_pwr.o(i.drv_pwr_set_pll_clk)
    i.drv_pwr_set_wakeup_type                0x00013f5c   Section        0  drv_pwr.o(i.drv_pwr_set_wakeup_type)
    i.drv_pwr_write_lock                     0x00013f88   Section        0  drv_pwr.o(i.drv_pwr_write_lock)
    i.drv_rxbr_clear_pkt_buffer              0x00013fa8   Section        0  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    i.drv_rxbr_clear_status0                 0x00013fb8   Section        0  drv_rxbr.o(i.drv_rxbr_clear_status0)
    i.drv_rxbr_enable_irq                    0x00013fc4   Section        0  drv_rxbr.o(i.drv_rxbr_enable_irq)
    i.drv_rxbr_frame_drop_cfg                0x00014020   Section        0  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    i.drv_rxbr_get_int_source                0x0001403c   Section        0  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    drv_rxbr_get_int_source                  0x0001403d   Thumb Code    20  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    i.drv_rxbr_get_status0                   0x00014054   Section        0  hal_internal_dcs.o(i.drv_rxbr_get_status0)
    drv_rxbr_get_status0                     0x00014055   Thumb Code    20  hal_internal_dcs.o(i.drv_rxbr_get_status0)
    i.drv_rxbr_hline_rcv1_cfg                0x0001406c   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg)
    i.drv_rxbr_hline_rcv_cfg                 0x00014080   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    i.drv_rxbr_register_irq1_callback        0x00014090   Section        0  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    i.drv_rxbr_set_cmd_response              0x0001409c   Section        0  drv_rxbr.o(i.drv_rxbr_set_cmd_response)
    i.drv_rxbr_set_color_format              0x000141e0   Section        0  drv_rxbr.o(i.drv_rxbr_set_color_format)
    i.drv_rxbr_set_filter_regs               0x000141fc   Section        0  drv_rxbr.o(i.drv_rxbr_set_filter_regs)
    i.drv_rxbr_set_inten                     0x00014220   Section        0  drv_rxbr.o(i.drv_rxbr_set_inten)
    i.drv_rxbr_set_ltpo_drop_th              0x0001423c   Section        0  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    i.drv_rxbr_set_usr_cfg                   0x00014254   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    i.drv_rxbr_set_usr_col                   0x00014294   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    i.drv_rxbr_set_usr_row                   0x000142a4   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    i.drv_se_init                            0x000142b4   Section        0  drv_se.o(i.drv_se_init)
    i.drv_se_set_dsc                         0x0001432c   Section        0  drv_se.o(i.drv_se_set_dsc)
    i.drv_se_set_lcdc                        0x00014400   Section        0  drv_se.o(i.drv_se_set_lcdc)
    i.drv_se_set_memc                        0x00014488   Section        0  drv_se.o(i.drv_se_set_memc)
    i.drv_se_set_rxbr                        0x00014518   Section        0  drv_se.o(i.drv_se_set_rxbr)
    i.drv_se_set_vidc                        0x000145e8   Section        0  drv_se.o(i.drv_se_set_vidc)
    i.drv_se_start_rx                        0x00014694   Section        0  drv_se.o(i.drv_se_start_rx)
    i.drv_spim_clear_int_status              0x000146a8   Section        0  drv_spi_master.o(i.drv_spim_clear_int_status)
    i.drv_spim_disable_int                   0x000146b4   Section        0  drv_spi_master.o(i.drv_spim_disable_int)
    i.drv_spim_get_busy                      0x000146e4   Section        0  drv_spi_master.o(i.drv_spim_get_busy)
    i.drv_spim_get_int_status                0x000146f4   Section        0  drv_spi_master.o(i.drv_spim_get_int_status)
    i.drv_spim_set_inten                     0x00014700   Section        0  drv_spi_master.o(i.drv_spim_set_inten)
    i.drv_swire_enable                       0x0001471c   Section        0  drv_swire.o(i.drv_swire_enable)
    i.drv_swire_get_pulse_count              0x00014738   Section        0  drv_swire.o(i.drv_swire_get_pulse_count)
    i.drv_swire_register_callback            0x00014744   Section        0  drv_swire.o(i.drv_swire_register_callback)
    i.drv_swire_set_bit_time                 0x00014750   Section        0  drv_swire.o(i.drv_swire_set_bit_time)
    i.drv_swire_set_int                      0x00014768   Section        0  drv_swire.o(i.drv_swire_set_int)
    i.drv_swire_set_power_down               0x000147b0   Section        0  drv_swire.o(i.drv_swire_set_power_down)
    i.drv_swire_set_pulse_count              0x000147cc   Section        0  drv_swire.o(i.drv_swire_set_pulse_count)
    i.drv_swire_set_trig_mode                0x000147d8   Section        0  drv_swire.o(i.drv_swire_set_trig_mode)
    i.drv_sys_cfg_clear_all_int              0x000147f4   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    i.drv_sys_cfg_clear_pending              0x00014800   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    i.drv_sys_cfg_sel_ap_rst_trig            0x00014828   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig)
    i.drv_sys_cfg_sel_gpio_group             0x0001484c   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group)
    i.drv_sys_cfg_sel_int_trig               0x00014870   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig)
    i.drv_sys_cfg_sel_swire_timer            0x00014894   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_swire_timer)
    i.drv_sys_cfg_set_int                    0x000148ac   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    i.drv_timer_clear_status_flags           0x000148d0   Section        0  drv_timer.o(i.drv_timer_clear_status_flags)
    drv_timer_clear_status_flags             0x000148d1   Thumb Code    26  drv_timer.o(i.drv_timer_clear_status_flags)
    i.drv_timer_enable                       0x000148ea   Section        0  drv_timer.o(i.drv_timer_enable)
    i.drv_timer_get_instance                 0x0001490c   Section        0  drv_timer.o(i.drv_timer_get_instance)
    i.drv_timer_handle_interrupt             0x0001491c   Section        0  drv_timer.o(i.drv_timer_handle_interrupt)
    drv_timer_handle_interrupt               0x0001491d   Thumb Code    54  drv_timer.o(i.drv_timer_handle_interrupt)
    i.drv_timer_register_callback            0x00014958   Section        0  drv_timer.o(i.drv_timer_register_callback)
    i.drv_timer_set_compare_val              0x0001496c   Section        0  drv_timer.o(i.drv_timer_set_compare_val)
    i.drv_timer_set_int                      0x000149ac   Section        0  drv_timer.o(i.drv_timer_set_int)
    i.drv_timer_set_prescaler                0x000149f4   Section        0  drv_timer.o(i.drv_timer_set_prescaler)
    i.drv_timer_set_repeat                   0x00014a1c   Section        0  drv_timer.o(i.drv_timer_set_repeat)
    i.drv_tx_phy_test_enter                  0x00014a2c   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    i.drv_tx_phy_test_exit                   0x00014a4c   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    i.drv_tx_phy_test_write_code             0x00014a6c   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    i.drv_uart_abort_recv                    0x00014a94   Section        0  drv_uart.o(i.drv_uart_abort_recv)
    i.drv_uart_abort_send                    0x00014ac8   Section        0  drv_uart.o(i.drv_uart_abort_send)
    i.drv_uart_config_int                    0x00014afc   Section        0  drv_uart.o(i.drv_uart_config_int)
    i.drv_uart_enable_clk                    0x00014b10   Section        0  drv_uart.o(i.drv_uart_enable_clk)
    drv_uart_enable_clk                      0x00014b11   Thumb Code    24  drv_uart.o(i.drv_uart_enable_clk)
    i.drv_uart_enable_int                    0x00014b28   Section        0  drv_uart.o(i.drv_uart_enable_int)
    i.drv_uart_get_instance                  0x00014b84   Section        0  drv_uart.o(i.drv_uart_get_instance)
    i.drv_uart_init                          0x00014bac   Section        0  drv_uart.o(i.drv_uart_init)
    i.drv_uart_int_trans_handle              0x00014c7c   Section        0  drv_uart.o(i.drv_uart_int_trans_handle)
    drv_uart_int_trans_handle                0x00014c7d   Thumb Code    54  drv_uart.o(i.drv_uart_int_trans_handle)
    i.drv_uart_reset_rx_fifo                 0x00014cb8   Section        0  drv_uart.o(i.drv_uart_reset_rx_fifo)
    i.drv_uart_reset_tx_fifo                 0x00014cd4   Section        0  drv_uart.o(i.drv_uart_reset_tx_fifo)
    i.drv_uart_send_blocking                 0x00014cf0   Section        0  drv_uart.o(i.drv_uart_send_blocking)
    i.drv_uart_set_baud_rate                 0x00014d0a   Section        0  drv_uart.o(i.drv_uart_set_baud_rate)
    i.drv_uart_trans_create_handle           0x00014d60   Section        0  drv_uart.o(i.drv_uart_trans_create_handle)
    i.drv_vidc_clear_irq                     0x00014dac   Section        0  drv_vidc.o(i.drv_vidc_clear_irq)
    i.drv_vidc_enable                        0x00014dbc   Section        0  drv_vidc.o(i.drv_vidc_enable)
    i.drv_vidc_enable_irq                    0x00014ddc   Section        0  drv_vidc.o(i.drv_vidc_enable_irq)
    i.drv_vidc_get_int_source                0x00014e1c   Section        0  drv_vidc.o(i.drv_vidc_get_int_source)
    i.drv_vidc_get_irq_status                0x00014e48   Section        0  drv_vidc.o(i.drv_vidc_get_irq_status)
    i.drv_vidc_init_module_enable            0x00014e60   Section        0  drv_vidc.o(i.drv_vidc_init_module_enable)
    i.drv_vidc_register_callback             0x00014e8c   Section        0  drv_vidc.o(i.drv_vidc_register_callback)
    i.drv_vidc_reset                         0x00014e98   Section        0  drv_vidc.o(i.drv_vidc_reset)
    i.drv_vidc_set_circ_mode_enable          0x00014ea4   Section        0  drv_vidc.o(i.drv_vidc_set_circ_mode_enable)
    i.drv_vidc_set_dither_config             0x00014ec0   Section        0  drv_vidc.o(i.drv_vidc_set_dither_config)
    i.drv_vidc_set_dst_parameter             0x00014ef8   Section        0  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    i.drv_vidc_set_honly_hcoef0              0x00014f54   Section        0  drv_vidc.o(i.drv_vidc_set_honly_hcoef0)
    i.drv_vidc_set_honly_hinitb              0x00014f60   Section        0  drv_vidc.o(i.drv_vidc_set_honly_hinitb)
    i.drv_vidc_set_honly_hinitr              0x00014f8c   Section        0  drv_vidc.o(i.drv_vidc_set_honly_hinitr)
    i.drv_vidc_set_irqen                     0x00014fbc   Section        0  drv_vidc.o(i.drv_vidc_set_irqen)
    i.drv_vidc_set_mirror                    0x00014fd8   Section        0  drv_vidc.o(i.drv_vidc_set_mirror)
    i.drv_vidc_set_pentile_swap              0x00014fec   Section        0  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    i.drv_vidc_set_pu_ctrl                   0x00015008   Section        0  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    i.drv_vidc_set_rotation                  0x00015014   Section        0  drv_vidc.o(i.drv_vidc_set_rotation)
    i.drv_vidc_set_scld_hcoef0               0x0001502c   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    i.drv_vidc_set_scld_hcoef1               0x00015038   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    i.drv_vidc_set_scld_step                 0x00015044   Section        0  drv_vidc.o(i.drv_vidc_set_scld_step)
    i.drv_vidc_set_scld_vcoef0               0x00015058   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    i.drv_vidc_set_scld_vcoef1               0x00015064   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    i.drv_vidc_set_src_parameter             0x00015070   Section        0  drv_vidc.o(i.drv_vidc_set_src_parameter)
    i.drv_vidc_set_vintp_config              0x00015090   Section        0  drv_vidc.o(i.drv_vidc_set_vintp_config)
    i.drv_wdg_clear_counter                  0x000150c8   Section        0  drv_wdg.o(i.drv_wdg_clear_counter)
    i.drv_wdg_clear_edge_flag                0x000150d8   Section        0  drv_wdg.o(i.drv_wdg_clear_edge_flag)
    drv_wdg_clear_edge_flag                  0x000150d9   Thumb Code    12  drv_wdg.o(i.drv_wdg_clear_edge_flag)
    i.drv_wdg_read_edge_flag                 0x000150e8   Section        0  drv_wdg.o(i.drv_wdg_read_edge_flag)
    drv_wdg_read_edge_flag                   0x000150e9   Thumb Code    10  drv_wdg.o(i.drv_wdg_read_edge_flag)
    i.drv_wdg_set_int                        0x000150f8   Section        0  drv_wdg.o(i.drv_wdg_set_int)
    i.fputc                                  0x0001512c   Section        0  tau_log.o(i.fputc)
    i.ha_intl_fb_check_pu_size               0x00015160   Section        0  hal_internal_fb.o(i.ha_intl_fb_check_pu_size)
    ha_intl_fb_check_pu_size                 0x00015161   Thumb Code    58  hal_internal_fb.o(i.ha_intl_fb_check_pu_size)
    i.hal_dsi_rx_ctrl_create_handle          0x000151a0   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    i.hal_dsi_rx_ctrl_dcs_async_handler      0x000151d8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler)
    i.hal_dsi_rx_ctrl_deinit                 0x00015218   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit)
    i.hal_dsi_rx_ctrl_init                   0x000152ac   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    i.hal_dsi_rx_ctrl_init_clk               0x00015340   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    hal_dsi_rx_ctrl_init_clk                 0x00015341   Thumb Code   222  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    i.hal_dsi_rx_ctrl_init_dsi_rx            0x00015440   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    hal_dsi_rx_ctrl_init_dsi_rx              0x00015441   Thumb Code   218  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    i.hal_dsi_rx_ctrl_init_memc              0x00015538   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    hal_dsi_rx_ctrl_init_memc                0x00015539   Thumb Code   294  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    i.hal_dsi_rx_ctrl_init_rxbr              0x00015664   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    hal_dsi_rx_ctrl_init_rxbr                0x00015665   Thumb Code   306  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    i.hal_dsi_rx_ctrl_init_vidc              0x000157a4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    hal_dsi_rx_ctrl_init_vidc                0x000157a5   Thumb Code   556  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    i.hal_dsi_rx_ctrl_pre_init_pps           0x000159e0   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    i.hal_dsi_rx_ctrl_set_auto_ack           0x00015a18   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack)
    i.hal_dsi_rx_ctrl_set_ipi_cfg            0x00015ac8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    hal_dsi_rx_ctrl_set_ipi_cfg              0x00015ac9   Thumb Code    48  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    i.hal_dsi_rx_ctrl_start                  0x00015af8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    i.hal_dsi_rx_ctrl_stop                   0x00015b28   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop)
    i.hal_dsi_rx_ctrl_toggle_resolution      0x00015b58   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    i.hal_dsi_tx_cmd_mode_cal_timing         0x00015b78   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing)
    hal_dsi_tx_cmd_mode_cal_timing           0x00015b79   Thumb Code   506  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing)
    i.hal_dsi_tx_ctrl_create_handle          0x00015df4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    i.hal_dsi_tx_ctrl_deinit                 0x00015e2c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit)
    i.hal_dsi_tx_ctrl_gen_a_tear_signal      0x00015e8c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal)
    i.hal_dsi_tx_ctrl_init                   0x00015eb0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    i.hal_dsi_tx_ctrl_init_clk               0x00015f24   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    hal_dsi_tx_ctrl_init_clk                 0x00015f25   Thumb Code    12  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    i.hal_dsi_tx_ctrl_set_overwrite_rgb      0x00015f34   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    i.hal_dsi_tx_ctrl_set_tear_mode          0x00015f3c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode)
    i.hal_dsi_tx_ctrl_start                  0x00015f48   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    i.hal_dsi_tx_ctrl_stop                   0x00015fb8   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop)
    i.hal_dsi_tx_ctrl_write_array_cmd        0x00015ff0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd)
    i.hal_dsi_tx_ctrl_write_cmd              0x000160e4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    i.hal_dsi_tx_init_cfg                    0x000161b4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg)
    hal_dsi_tx_init_cfg                      0x000161b5   Thumb Code   258  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg)
    i.hal_dsi_tx_init_dpi_timing             0x000162c0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing)
    hal_dsi_tx_init_dpi_timing               0x000162c1   Thumb Code    46  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing)
    i.hal_dsi_tx_init_phy_cfg                0x000162f8   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    hal_dsi_tx_init_phy_cfg                  0x000162f9   Thumb Code    22  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    i.hal_dsi_tx_init_timing                 0x0001630e   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing)
    hal_dsi_tx_init_timing                   0x0001630f   Thumb Code    82  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing)
    i.hal_dsi_tx_init_vid_timing             0x00016360   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing)
    hal_dsi_tx_init_vid_timing               0x00016361   Thumb Code    70  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing)
    i.hal_dsi_tx_send_cmd                    0x000163b4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    hal_dsi_tx_send_cmd                      0x000163b5   Thumb Code    50  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    i.hal_dsi_tx_timing_info_update          0x000163ec   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update)
    hal_dsi_tx_timing_info_update            0x000163ed   Thumb Code   128  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update)
    i.hal_dsi_tx_vid_mode_cal_timing         0x00016470   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing)
    hal_dsi_tx_vid_mode_cal_timing           0x00016471   Thumb Code   766  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing)
    i.hal_gpio_config_pad                    0x00016780   Section        0  hal_gpio.o(i.hal_gpio_config_pad)
    i.hal_gpio_ctrl_eint                     0x000167bc   Section        0  hal_gpio.o(i.hal_gpio_ctrl_eint)
    i.hal_gpio_init_eint                     0x000167d4   Section        0  hal_gpio.o(i.hal_gpio_init_eint)
    i.hal_gpio_init_input                    0x00016814   Section        0  hal_gpio.o(i.hal_gpio_init_input)
    i.hal_gpio_init_output                   0x00016838   Section        0  hal_gpio.o(i.hal_gpio_init_output)
    i.hal_gpio_reg_eint_cb                   0x00016860   Section        0  hal_gpio.o(i.hal_gpio_reg_eint_cb)
    i.hal_gpio_set_ap_reset_int              0x00016878   Section        0  hal_gpio.o(i.hal_gpio_set_ap_reset_int)
    i.hal_gpio_set_mode                      0x000168c8   Section        0  hal_gpio.o(i.hal_gpio_set_mode)
    i.hal_gpio_set_output_data               0x0001692c   Section        0  hal_gpio.o(i.hal_gpio_set_output_data)
    i.hal_gpio_set_pull_state                0x00016934   Section        0  hal_gpio.o(i.hal_gpio_set_pull_state)
    i.hal_internal_sync_get_hight_performan_mode 0x0001697c   Section        0  hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode)
    i.hal_internal_sync_input_resolution_change 0x0001698c   Section        0  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    i.hal_internal_sync_register_lcdc_cb     0x00016b3c   Section        0  hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb)
    i.hal_internal_vsync_deinit              0x00016b48   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    i.hal_internal_vsync_get_rx_state        0x00016b68   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state)
    i.hal_internal_vsync_get_sync_line       0x00016b74   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    i.hal_internal_vsync_get_tx_state        0x00016b8c   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    i.hal_internal_vsync_init_rx             0x00016b98   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    i.hal_internal_vsync_init_tx             0x00016c70   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    i.hal_internal_vsync_set_rx_state        0x00016d34   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    i.hal_internal_vsync_set_tear_mode       0x00016d54   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    i.hal_internal_vsync_set_tx_state        0x00016e4c   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    i.hal_intl_dcs_init_sw_fltr              0x00016eb8   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr)
    i.hal_intl_dcs_rx_get_dcs_packet_data    0x00016f24   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data)
    hal_intl_dcs_rx_get_dcs_packet_data      0x00016f25   Thumb Code   806  hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data)
    i.hal_intl_dcs_rx_receive_packet         0x00017370   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet)
    hal_intl_dcs_rx_receive_packet           0x00017371   Thumb Code   122  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet)
    i.hal_intl_dcs_rx_receive_pps            0x000173f8   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps)
    hal_intl_dcs_rx_receive_pps              0x000173f9   Thumb Code   268  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps)
    i.hal_intl_dcs_set_auto_hw_filter        0x0001756c   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter)
    i.hal_intl_dcs_sw_filter_handle          0x000175f8   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle)
    hal_intl_dcs_sw_filter_handle            0x000175f9   Thumb Code    36  hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle)
    i.hal_intl_fb_cal_fb_info                0x00017624   Section        0  hal_internal_fb.o(i.hal_intl_fb_cal_fb_info)
    i.hal_intl_fb_check_bandwidth            0x00017904   Section        0  hal_internal_fb.o(i.hal_intl_fb_check_bandwidth)
    hal_intl_fb_check_bandwidth              0x00017905   Thumb Code    92  hal_internal_fb.o(i.hal_intl_fb_check_bandwidth)
    i.hal_intl_fb_edge_resize                0x00017968   Section        0  hal_internal_fb.o(i.hal_intl_fb_edge_resize)
    hal_intl_fb_edge_resize                  0x00017969   Thumb Code   194  hal_internal_fb.o(i.hal_intl_fb_edge_resize)
    i.hal_intl_fb_flow_control_adapter       0x00017a30   Section        0  hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter)
    hal_intl_fb_flow_control_adapter         0x00017a31   Thumb Code    94  hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter)
    i.hal_intl_fb_get_memc_flow_mode         0x00017a94   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode)
    i.hal_intl_fb_get_rx_fb_info             0x00017aa0   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info)
    i.hal_intl_fb_get_tx_fb_info             0x00017ab0   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info)
    i.hal_intl_fb_get_user_flow              0x00017ac0   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_user_flow)
    i.hal_intl_svs_deinit_rx                 0x00017acc   Section        0  hal_internal_svs.o(i.hal_intl_svs_deinit_rx)
    i.hal_intl_svs_deinit_tx                 0x00017af4   Section        0  hal_internal_svs.o(i.hal_intl_svs_deinit_tx)
    i.hal_intl_svs_handle                    0x00017b04   Section        0  hal_internal_svs.o(i.hal_intl_svs_handle)
    i.hal_intl_svs_init_rx                   0x00017b28   Section        0  hal_internal_svs.o(i.hal_intl_svs_init_rx)
    i.hal_intl_svs_init_tx                   0x00017ba8   Section        0  hal_internal_svs.o(i.hal_intl_svs_init_tx)
    i.hal_intl_svs_set_rx_vtt                0x00017bbc   Section        0  hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt)
    i.hal_intl_svs_update_rxbr_clk           0x00017bc8   Section        0  hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk)
    i.hal_lcdc_displayproc_config            0x00017c10   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config)
    i.hal_lcdc_func_update                   0x00017c80   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_func_update)
    i.hal_lcdc_init_cfg                      0x00017ce4   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    hal_lcdc_init_cfg                        0x00017ce5   Thumb Code    62  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    i.hal_lcdc_init_clk                      0x00017d22   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    hal_lcdc_init_clk                        0x00017d23   Thumb Code   112  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    i.hal_lcdc_postproc_config               0x00017d94   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config)
    i.hal_lcdc_start                         0x00017ebc   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_start)
    hal_lcdc_start                           0x00017ebd   Thumb Code    36  hal_dsi_tx_ctrl.o(i.hal_lcdc_start)
    i.hal_lcdc_timinggen_config              0x00017ee0   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config)
    hal_lcdc_timinggen_config                0x00017ee1   Thumb Code    60  hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config)
    i.hal_lcdc_upscaler_config               0x00017f1c   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config)
    i.hal_pwr_enter_deep_sleep_mode          0x00017ff0   Section        0  hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode)
    i.hal_pwr_enter_normal_sleep_mode        0x0001801a   Section        0  hal_pwr.o(i.hal_pwr_enter_normal_sleep_mode)
    i.hal_pwr_enter_stop_sleep_mode          0x00018024   Section        0  hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode)
    i.hal_pwr_exit_sleep_mode                0x00018088   Section        0  hal_pwr.o(i.hal_pwr_exit_sleep_mode)
    i.hal_pwr_get_vcc_power_ready            0x00018092   Section        0  hal_pwr.o(i.hal_pwr_get_vcc_power_ready)
    i.hal_pwr_set_main_power                 0x0001809a   Section        0  hal_pwr.o(i.hal_pwr_set_main_power)
    i.hal_pwr_set_sleep_mode_power           0x000180a2   Section        0  hal_pwr.o(i.hal_pwr_set_sleep_mode_power)
    i.hal_pwr_set_stop_sleep_wakeup_pin      0x000180ac   Section        0  hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin)
    i.hal_swire_deinit                       0x00018110   Section        0  hal_swire.o(i.hal_swire_deinit)
    i.hal_swire_enable                       0x00018150   Section        0  hal_swire.o(i.hal_swire_enable)
    i.hal_swire_init                         0x000181ac   Section        0  hal_swire.o(i.hal_swire_init)
    i.hal_swire_set_pulse                    0x00018204   Section        0  hal_swire.o(i.hal_swire_set_pulse)
    i.hal_swire_set_timer                    0x00018228   Section        0  hal_swire.o(i.hal_swire_set_timer)
    i.hal_system_init                        0x00018268   Section        0  hal_system.o(i.hal_system_init)
    i.hal_timer_deinit                       0x00018380   Section        0  hal_timer.o(i.hal_timer_deinit)
    i.hal_timer_init                         0x000183b0   Section        0  hal_timer.o(i.hal_timer_init)
    i.hal_timer_set_repeat                   0x000183cc   Section        0  hal_timer.o(i.hal_timer_set_repeat)
    i.hal_timer_start                        0x000183d4   Section        0  hal_timer.o(i.hal_timer_start)
    i.hal_timer_stop                         0x00018404   Section        0  hal_timer.o(i.hal_timer_stop)
    i.hal_tx_frame_rate_adjust               0x0001842c   Section        0  hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust)
    hal_tx_frame_rate_adjust                 0x0001842d   Thumb Code    44  hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust)
    i.hal_uart_init                          0x0001845c   Section        0  hal_uart.o(i.hal_uart_init)
    i.hal_uart_send_blocking                 0x000184f0   Section        0  hal_uart.o(i.hal_uart_send_blocking)
    i.hal_vsync_reset_lcdc_scaler            0x0001850c   Section        0  hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler)
    i.main                                   0x000185d8   Section        0  main.o(i.main)
    i.pps_update_handle                      0x00018618   Section        0  s8_demo.o(i.pps_update_handle)
    pps_update_handle                        0x00018619   Thumb Code    76  s8_demo.o(i.pps_update_handle)
    i.rxbr_irq1_callback                     0x0001866c   Section        0  hal_internal_vsync.o(i.rxbr_irq1_callback)
    rxbr_irq1_callback                       0x0001866d   Thumb Code   456  hal_internal_vsync.o(i.rxbr_irq1_callback)
    i.s8_demo                                0x00018918   Section        0  s8_demo.o(i.s8_demo)
    i.send_panel_init_code                   0x00018978   Section        0  s8_demo.o(i.send_panel_init_code)
    send_panel_init_code                     0x00018979   Thumb Code    58  s8_demo.o(i.send_panel_init_code)
    i.soft_double_buffer_update              0x000189b4   Section        0  hal_internal_vsync.o(i.soft_double_buffer_update)
    soft_double_buffer_update                0x000189b5   Thumb Code    56  hal_internal_vsync.o(i.soft_double_buffer_update)
    i.soft_gen_te                            0x000189f8   Section        0  hal_internal_vsync.o(i.soft_gen_te)
    soft_gen_te                              0x000189f9   Thumb Code    52  hal_internal_vsync.o(i.soft_gen_te)
    i.soft_gen_te_double_buffer              0x00018a3c   Section        0  hal_internal_vsync.o(i.soft_gen_te_double_buffer)
    soft_gen_te_double_buffer                0x00018a3d   Thumb Code    66  hal_internal_vsync.o(i.soft_gen_te_double_buffer)
    i.soft_swire_init                        0x00018a90   Section        0  s8_demo.o(i.soft_swire_init)
    soft_swire_init                          0x00018a91   Thumb Code    48  s8_demo.o(i.soft_swire_init)
    i.soft_swire_start                       0x00018ac8   Section        0  s8_demo.o(i.soft_swire_start)
    soft_swire_start                         0x00018ac9   Thumb Code    46  s8_demo.o(i.soft_swire_start)
    i.soft_swire_timer_callback              0x00018af8   Section        0  s8_demo.o(i.soft_swire_timer_callback)
    soft_swire_timer_callback                0x00018af9   Thumb Code    64  s8_demo.o(i.soft_swire_timer_callback)
    i.stop_sleep_cb                          0x00018b40   Section        0  hal_pwr.o(i.stop_sleep_cb)
    stop_sleep_cb                            0x00018b41   Thumb Code    18  hal_pwr.o(i.stop_sleep_cb)
    i.svs_direct_mode_setting                0x00018b58   Section        0  hal_internal_svs.o(i.svs_direct_mode_setting)
    svs_direct_mode_setting                  0x00018b59   Thumb Code   154  hal_internal_svs.o(i.svs_direct_mode_setting)
    i.svs_get_rel_intv                       0x00018c04   Section        0  hal_internal_svs.o(i.svs_get_rel_intv)
    svs_get_rel_intv                         0x00018c05   Thumb Code    20  hal_internal_svs.o(i.svs_get_rel_intv)
    i.svs_sync_handle                        0x00018c20   Section        0  hal_internal_svs.o(i.svs_sync_handle)
    svs_sync_handle                          0x00018c21   Thumb Code   158  hal_internal_svs.o(i.svs_sync_handle)
    i.svs_wait_fr_stab                       0x00018cd0   Section        0  hal_internal_svs.o(i.svs_wait_fr_stab)
    svs_wait_fr_stab                         0x00018cd1   Thumb Code   148  hal_internal_svs.o(i.svs_wait_fr_stab)
    i.svs_wait_start                         0x00018d9c   Section        0  hal_internal_svs.o(i.svs_wait_start)
    svs_wait_start                           0x00018d9d   Thumb Code   250  hal_internal_svs.o(i.svs_wait_start)
    i.tau_log_init                           0x00018ea8   Section        0  tau_log.o(i.tau_log_init)
    i.tau_log_printf                         0x00018edc   Section        0  tau_log.o(i.tau_log_printf)
    i.tau_log_push_log                       0x00018f60   Section        0  tau_log.o(i.tau_log_push_log)
    i.vidc_callback                          0x00018fd8   Section        0  hal_internal_vsync.o(i.vidc_callback)
    vidc_callback                            0x00018fd9   Thumb Code   150  hal_internal_vsync.o(i.vidc_callback)
    i.vpre_err_reset                         0x0001908c   Section        0  hal_internal_vsync.o(i.vpre_err_reset)
    vpre_err_reset                           0x0001908d   Thumb Code   232  hal_internal_vsync.o(i.vpre_err_reset)
    .constdata                               0x000191bc   Section     7932  s8_demo.o(.constdata)
    g_cus_rx_dcs_execute_table               0x000191bc   Data          96  s8_demo.o(.constdata)
    .constdata                               0x0001b0b8   Section       40  hal_dsi_rx_ctrl.o(.constdata)
    .constdata                               0x0001b0e0   Section       28  hal_dsi_tx_ctrl.o(.constdata)
    .constdata                               0x0001b0fc   Section      208  hal_gpio.o(.constdata)
    s_gpio_map                               0x0001b0fc   Data         130  hal_gpio.o(.constdata)
    s_gpio_perf                              0x0001b17e   Data          78  hal_gpio.o(.constdata)
    .constdata                               0x0001b1cc   Section       48  hal_uart.o(.constdata)
    .constdata                               0x0001b1fc   Section       16  drv_uart.o(.constdata)
    .conststring                             0x0001b20c   Section      135  hal_dsi_rx_ctrl.o(.conststring)
    .conststring                             0x0001b294   Section      142  hal_internal_vsync.o(.conststring)
    .conststring                             0x0001b324   Section      142  hal_internal_dcs.o(.conststring)
    .data                                    0x00070000   Section      142  s8_demo.o(.data)
    g_rx_ctrl_handle                         0x00070000   Data           4  s8_demo.o(.data)
    g_tx_ctrl_handle                         0x00070004   Data           4  s8_demo.o(.data)
    panel_display_done                       0x00070008   Data           1  s8_demo.o(.data)
    sg_system_resume                         0x00070009   Data           1  s8_demo.o(.data)
    sg_system_suspend                        0x0007000a   Data           1  s8_demo.o(.data)
    AP_REG51_7FF                             0x0007000b   Data           1  s8_demo.o(.data)
    sg_tx_start_in_process                   0x0007000c   Data           1  s8_demo.o(.data)
    .data                                    0x00070090   Section        8  hal_dsi_rx_ctrl.o(.data)
    g_hw_auto_filter                         0x00070090   Data           1  hal_dsi_rx_ctrl.o(.data)
    g_crc_check_enable                       0x00070091   Data           1  hal_dsi_rx_ctrl.o(.data)
    g_esc_clk                                0x00070094   Data           4  hal_dsi_rx_ctrl.o(.data)
    .data                                    0x00070098   Section       92  hal_dsi_tx_ctrl.o(.data)
    sg_bta_vsync_flag                        0x00070098   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_vsync_flag                            0x00070099   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_enter_sleep_cmd                       0x0007009a   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_fldc_cg_mode                          0x0007009b   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_scl_fir                        0x0007009c   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_honly_bypass_fir                      0x0007009d   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_bcs                            0x0007009e   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_enhc                           0x0007009f   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_edge_dect                      0x000700a0   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_edge_enh                       0x000700a1   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_dith                           0x000700a2   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_dith_judge                            0x000700a3   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_endianness                            0x000700a4   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_dith_judge_thr                        0x000700a8   Data           4  hal_dsi_tx_ctrl.o(.data)
    sg_ccm_para                              0x000700ac   Data          36  hal_dsi_tx_ctrl.o(.data)
    sg_honly_para                            0x000700d0   Data          36  hal_dsi_tx_ctrl.o(.data)
    .data                                    0x000700f4   Section        1  hal_spi_master.o(.data)
    sg_spim_trans_end                        0x000700f4   Data           1  hal_spi_master.o(.data)
    .data                                    0x000700f5   Section        2  hal_swire.o(.data)
    sg_swire_timer                           0x000700f5   Data           1  hal_swire.o(.data)
    sg_swire_repeat                          0x000700f6   Data           1  hal_swire.o(.data)
    .data                                    0x000700f8   Section        8  hal_pwr.o(.data)
    sg_wake_up_io                            0x000700f8   Data           1  hal_pwr.o(.data)
    sg_stop_sleep_wakeup_int                 0x000700fc   Data           4  hal_pwr.o(.data)
    .data                                    0x00070100   Section        1  tau_log.o(.data)
    g_log_port                               0x00070100   Data           1  tau_log.o(.data)
    .data                                    0x00070104   Section       24  hal_uart.o(.data)
    sg_dma_callback                          0x00070114   Data           4  hal_uart.o(.data)
    sg_user_data                             0x00070118   Data           4  hal_uart.o(.data)
    .data                                    0x0007011c   Section        8  hal_internal_vsync.o(.data)
    .data                                    0x00070124   Section       36  hal_internal_dcs.o(.data)
    g_imm_packet                             0x00070124   Data          24  hal_internal_dcs.o(.data)
    g_cus_rx_write_cmd_handle                0x0007013c   Data          12  hal_internal_dcs.o(.data)
    .data                                    0x00070148   Section       12  drv_common.o(.data)
    s_my_tick                                0x00070148   Data           4  drv_common.o(.data)
    .data                                    0x00070154   Section        1  drv_common.o(.data)
    .data                                    0x00070158   Section      400  drv_dma.o(.data)
    sg_dma_handle                            0x00070158   Data         256  drv_dma.o(.data)
    .data                                    0x000702e8   Section        4  drv_gpio.o(.data)
    g_ap_reset_cb                            0x000702e8   Data           4  drv_gpio.o(.data)
    .data                                    0x000702ec   Section        4  drv_swire.o(.data)
    sg_drv_swire_cb                          0x000702ec   Data           4  drv_swire.o(.data)
    .data                                    0x000702f0   Section       80  drv_timer.o(.data)
    sg_timer_info                            0x000702f0   Data          80  drv_timer.o(.data)
    .data                                    0x00070340   Section       12  drv_wdg.o(.data)
    sg_wdg_repeat                            0x00070340   Data           1  drv_wdg.o(.data)
    sg_wdg_cb                                0x00070344   Data           8  drv_wdg.o(.data)
    .data                                    0x0007034c   Section       60  drv_i2c.o(.data)
    .data                                    0x00070388   Section        4  drv_se.o(.data)
    chip_info                                0x00070388   Data           4  drv_se.o(.data)
    .data                                    0x0007038c   Section        1  drv_dsi_rx.o(.data)
    sg_rx_drv_level                          0x0007038c   Data           1  drv_dsi_rx.o(.data)
    .data                                    0x00070390   Section        8  drv_rxbr.o(.data)
    .data                                    0x00070398   Section        4  drv_vidc.o(.data)
    .data                                    0x0007039c   Section        4  stdout.o(.data)
    .bss                                     0x000703a0   Section      204  hal_dsi_rx_ctrl.o(.bss)
    g_rx_ctrl_handle                         0x000703a0   Data         204  hal_dsi_rx_ctrl.o(.bss)
    .bss                                     0x0007046c   Section      180  hal_dsi_tx_ctrl.o(.bss)
    g_tx_ctrl_handle                         0x0007046c   Data          88  hal_dsi_tx_ctrl.o(.bss)
    sg_dsi_tx_param                          0x000704c4   Data          92  hal_dsi_tx_ctrl.o(.bss)
    .bss                                     0x00070520   Section      256  tau_log.o(.bss)
    g_log_buf                                0x00070520   Data         256  tau_log.o(.bss)
    .bss                                     0x00070620   Section       36  hal_internal_vsync.o(.bss)
    .bss                                     0x00070644   Section     2048  hal_internal_dcs.o(.bss)
    .bss                                     0x00070e44   Section      255  hal_internal_dcs.o(.bss)
    g_imm_buffer                             0x00070e44   Data         255  hal_internal_dcs.o(.bss)
    .bss                                     0x00070f44   Section       68  hal_internal_fb.o(.bss)
    .bss                                     0x00070f88   Section       68  hal_internal_svs.o(.bss)
    sg_sys_handler                           0x00070f88   Data          68  hal_internal_svs.o(.bss)
    .bss                                     0x00070fcc   Section       16  drv_dma.o(.bss)
    sg_dma_int_list                          0x00070fcc   Data          16  drv_dma.o(.bss)
    .bss                                     0x00070fdc   Section       64  drv_gpio.o(.bss)
    s_gpio_cb                                0x00070fdc   Data          64  drv_gpio.o(.bss)
    .bss                                     0x0007101c   Section     4204  dcs_packet_fifo.o(.bss)
    .bss                                     0x00072088   Section       96  drv_uart.o(.bss)
    sg_uart_userdata                         0x00072088   Data          96  drv_uart.o(.bss)
    STACK                                    0x000720e8   Section     4096  startup_armcm0.o(STACK)

    Global Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    BuildAttributes$$THM_ISAv3M$S$PE$A:L22$X:L11$S22$IEEE1$IW$USESV6$~STKCKD$USESV7$~SHL$OTIME$ROPI$IEEEJ$EBA8$MICROLIB$REQ8$PRES8$EABIv2 0x00000000   Number         0  anon$$obj.o ABSOLUTE
    __ARM_use_no_argv                        0x00000000   Number         0  main.o ABSOLUTE
    _printf_a                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_c                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_charcount                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_d                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_e                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_f                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_flags                            0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_dec                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_hex                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_g                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_i                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_int_dec                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_l                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ll                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lld                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lli                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llo                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llu                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llx                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_dec                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_hex                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_oct                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ls                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_mbtowc                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_n                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_o                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_p                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_percent                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_pre_padding                      0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_return_value                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_s                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_sizespec                         0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_str                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_signed                  0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_unsigned                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_u                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wctomb                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_widthprec                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_x                                0x00000000   Number         0  stubs.o ABSOLUTE
    __cpp_initialize__aeabi_                  - Undefined Weak Reference
    __cxa_finalize                            - Undefined Weak Reference
    _clock_init                               - Undefined Weak Reference
    _microlib_exit                            - Undefined Weak Reference
    __Vectors_Size                           0x000000c0   Number         0  startup_armcm0.o ABSOLUTE
    __Vectors                                0x00010000   Data           4  startup_armcm0.o(RESET)
    __Vectors_End                            0x000100c0   Data           0  startup_armcm0.o(RESET)
    __main                                   0x000100c1   Thumb Code     0  entry.o(.ARM.Collect$$$$00000000)
    _main_stk                                0x000100c1   Thumb Code     0  entry2.o(.ARM.Collect$$$$00000001)
    _main_scatterload                        0x000100c5   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    __main_after_scatterload                 0x000100c9   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    _main_clock                              0x000100c9   Thumb Code     0  entry7b.o(.ARM.Collect$$$$00000008)
    _main_cpp_init                           0x000100c9   Thumb Code     0  entry8b.o(.ARM.Collect$$$$0000000A)
    _main_init                               0x000100c9   Thumb Code     0  entry9a.o(.ARM.Collect$$$$0000000B)
    __rt_final_cpp                           0x000100d1   Thumb Code     0  entry10a.o(.ARM.Collect$$$$0000000D)
    __rt_final_exit                          0x000100d1   Thumb Code     0  entry11a.o(.ARM.Collect$$$$0000000F)
    Reset_Handler                            0x000100d5   Thumb Code    28  startup_armcm0.o(.text)
    NMI_Handler                              0x000100f1   Thumb Code     2  startup_armcm0.o(.text)
    SVC_Handler                              0x000100f5   Thumb Code     2  startup_armcm0.o(.text)
    PendSV_Handler                           0x000100f7   Thumb Code     2  startup_armcm0.o(.text)
    FLSCTRL_IRQn_Handler                     0x00010107   Thumb Code     2  startup_armcm0.o(.text)
    SPIS_IRQn_Handler                        0x0001011b   Thumb Code     2  startup_armcm0.o(.text)
    OTP_IRQn_Handler                         0x00010123   Thumb Code     2  startup_armcm0.o(.text)
    PVD_IRQn_Handler                         0x00010127   Thumb Code     2  startup_armcm0.o(.text)
    __aeabi_uidiv                            0x0001014d   Thumb Code     0  uidiv.o(.text)
    __aeabi_uidivmod                         0x0001014d   Thumb Code    44  uidiv.o(.text)
    __aeabi_idiv                             0x00010179   Thumb Code     0  idiv.o(.text)
    __aeabi_idivmod                          0x00010179   Thumb Code    40  idiv.o(.text)
    __aeabi_memcpy                           0x000101a1   Thumb Code    36  memcpya.o(.text)
    __aeabi_memcpy4                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memcpy8                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memset                           0x000101c5   Thumb Code    14  memseta.o(.text)
    __aeabi_memset4                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memset8                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr                           0x000101d3   Thumb Code     4  memseta.o(.text)
    __aeabi_memclr4                          0x000101d3   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr8                          0x000101d3   Thumb Code     0  memseta.o(.text)
    _memset$wrapper                          0x000101d7   Thumb Code    18  memseta.o(.text)
    strlen                                   0x000101e9   Thumb Code    14  strlen.o(.text)
    __aeabi_fadd                             0x000101f7   Thumb Code   162  fadd.o(.text)
    __aeabi_fsub                             0x00010299   Thumb Code     8  fadd.o(.text)
    __aeabi_frsub                            0x000102a1   Thumb Code     8  fadd.o(.text)
    __aeabi_fmul                             0x000102a9   Thumb Code   122  fmul.o(.text)
    __aeabi_fdiv                             0x00010323   Thumb Code   124  fdiv.o(.text)
    __ARM_scalbnf                            0x0001039f   Thumb Code    24  fscalb.o(.text)
    scalbnf                                  0x0001039f   Thumb Code     0  fscalb.o(.text)
    __aeabi_dadd                             0x000103b9   Thumb Code   328  dadd.o(.text)
    __aeabi_dsub                             0x00010501   Thumb Code    12  dadd.o(.text)
    __aeabi_drsub                            0x0001050d   Thumb Code    12  dadd.o(.text)
    __aeabi_dmul                             0x0001051d   Thumb Code   202  dmul.o(.text)
    __aeabi_ddiv                             0x000105ed   Thumb Code   234  ddiv.o(.text)
    __aeabi_ui2f                             0x000106dd   Thumb Code    14  ffltui.o(.text)
    __aeabi_ui2d                             0x000106ed   Thumb Code    24  dfltui.o(.text)
    __aeabi_f2uiz                            0x00010709   Thumb Code    40  ffixui.o(.text)
    __aeabi_d2uiz                            0x00010731   Thumb Code    50  dfixui.o(.text)
    __aeabi_f2d                              0x0001076d   Thumb Code    40  f2d.o(.text)
    __aeabi_d2f                              0x00010795   Thumb Code    56  d2f.o(.text)
    __aeabi_cfcmpeq                          0x000107cd   Thumb Code     0  cfcmple.o(.text)
    __aeabi_cfcmple                          0x000107cd   Thumb Code    20  cfcmple.o(.text)
    __aeabi_cfrcmple                         0x000107e1   Thumb Code    20  cfrcmple.o(.text)
    __aeabi_uldivmod                         0x000107f5   Thumb Code    96  uldiv.o(.text)
    __aeabi_llsl                             0x00010855   Thumb Code    32  llshl.o(.text)
    _ll_shift_l                              0x00010855   Thumb Code     0  llshl.o(.text)
    __aeabi_llsr                             0x00010875   Thumb Code    34  llushr.o(.text)
    _ll_ushift_r                             0x00010875   Thumb Code     0  llushr.o(.text)
    __aeabi_lasr                             0x00010897   Thumb Code    38  llsshr.o(.text)
    _ll_sshift_r                             0x00010897   Thumb Code     0  llsshr.o(.text)
    __I$use$fp                               0x000108bd   Thumb Code     0  iusefp.o(.text)
    _float_round                             0x000108bd   Thumb Code    16  fepilogue.o(.text)
    _float_epilogue                          0x000108cd   Thumb Code   114  fepilogue.o(.text)
    _double_round                            0x0001093f   Thumb Code    26  depilogue.o(.text)
    _double_epilogue                         0x00010959   Thumb Code   164  depilogue.o(.text)
    __aeabi_d2ulz                            0x000109fd   Thumb Code    54  dfixul.o(.text)
    __aeabi_cdrcmple                         0x00010a3d   Thumb Code    38  cdrcmple.o(.text)
    __scatterload                            0x00010a65   Thumb Code    28  init.o(.text)
    __scatterload_rt2                        0x00010a65   Thumb Code     0  init.o(.text)
    __decompress                             0x00010a89   Thumb Code     0  __dczerorl2.o(.text)
    __decompress1                            0x00010a89   Thumb Code    86  __dczerorl2.o(.text)
    AP_NRESET_IRQn_Handler                   0x00010ae1   Thumb Code    22  drv_gpio.o(i.AP_NRESET_IRQn_Handler)
    DMA_IRQn_Handler                         0x00010afd   Thumb Code    78  drv_dma.o(i.DMA_IRQn_Handler)
    EXTI_INT0_IRQn_Handler                   0x00010b59   Thumb Code    10  drv_gpio.o(i.EXTI_INT0_IRQn_Handler)
    EXTI_INT1_IRQn_Handler                   0x00010b63   Thumb Code    10  drv_gpio.o(i.EXTI_INT1_IRQn_Handler)
    EXTI_INT2_IRQn_Handler                   0x00010b6d   Thumb Code    10  drv_gpio.o(i.EXTI_INT2_IRQn_Handler)
    EXTI_INT3_IRQn_Handler                   0x00010b77   Thumb Code    10  drv_gpio.o(i.EXTI_INT3_IRQn_Handler)
    EXTI_INT4_IRQn_Handler                   0x00010b81   Thumb Code    10  drv_gpio.o(i.EXTI_INT4_IRQn_Handler)
    EXTI_INT5_IRQn_Handler                   0x00010b8b   Thumb Code    10  drv_gpio.o(i.EXTI_INT5_IRQn_Handler)
    EXTI_INT6_IRQn_Handler                   0x00010b95   Thumb Code    10  drv_gpio.o(i.EXTI_INT6_IRQn_Handler)
    EXTI_INT7_IRQn_Handler                   0x00010b9f   Thumb Code    10  drv_gpio.o(i.EXTI_INT7_IRQn_Handler)
    HardFault_Handler                        0x00010ba9   Thumb Code    14  drv_common.o(i.HardFault_Handler)
    I2C0_IRQn_Handler                        0x00010bf1   Thumb Code     8  drv_i2c.o(i.I2C0_IRQn_Handler)
    I2C1_IRQn_Handler                        0x00010bfd   Thumb Code     8  drv_i2c.o(i.I2C1_IRQn_Handler)
    I2C2_IRQn_Handler                        0x00010c09   Thumb Code     8  drv_i2c.o(i.I2C2_IRQn_Handler)
    LCDC_IRQn_Handler                        0x00010c15   Thumb Code    96  hal_internal_vsync.o(i.LCDC_IRQn_Handler)
    MEMC_IRQn_Handler                        0x00010cfd   Thumb Code   154  drv_memc.o(i.MEMC_IRQn_Handler)
    MIPI_TX_IRQn_Handler                     0x00010d99   Thumb Code    70  drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler)
    SPIM_IRQn_Handler                        0x00010e51   Thumb Code    60  hal_spi_master.o(i.SPIM_IRQn_Handler)
    SWIRE_IRQn_Handler                       0x00010e91   Thumb Code    38  drv_swire.o(i.SWIRE_IRQn_Handler)
    SysTick_Handler                          0x00010ec1   Thumb Code    20  drv_common.o(i.SysTick_Handler)
    TIMER0_IRQn_Handler                      0x00010ed9   Thumb Code    10  drv_timer.o(i.TIMER0_IRQn_Handler)
    TIMER1_IRQn_Handler                      0x00010ee3   Thumb Code    10  drv_timer.o(i.TIMER1_IRQn_Handler)
    TIMER2_IRQn_Handler                      0x00010eed   Thumb Code    10  drv_timer.o(i.TIMER2_IRQn_Handler)
    TIMER3_IRQn_Handler                      0x00010ef7   Thumb Code    10  drv_timer.o(i.TIMER3_IRQn_Handler)
    VIDC_IRQn_Handler                        0x00010f01   Thumb Code    22  drv_vidc.o(i.VIDC_IRQn_Handler)
    VPRE1_IRQn_Handler                       0x00010f1d   Thumb Code    22  drv_rxbr.o(i.VPRE1_IRQn_Handler)
    VPRE_IRQn_Handler                        0x00010f39   Thumb Code   104  hal_internal_dcs.o(i.VPRE_IRQn_Handler)
    WDG_IRQn_Handler                         0x00010fa5   Thumb Code    52  drv_wdg.o(i.WDG_IRQn_Handler)
    __0printf                                0x00010fdd   Thumb Code    24  printfa.o(i.__0printf)
    __1printf                                0x00010fdd   Thumb Code     0  printfa.o(i.__0printf)
    __2printf                                0x00010fdd   Thumb Code     0  printfa.o(i.__0printf)
    __c89printf                              0x00010fdd   Thumb Code     0  printfa.o(i.__0printf)
    printf                                   0x00010fdd   Thumb Code     0  printfa.o(i.__0printf)
    __scatterload_null                       0x00010ffd   Thumb Code     2  handlers.o(i.__scatterload_null)
    s_RAM_CK                                 0x00011000   Data          28  drv_common.o(.ARM.__at_0x11000)
    g_tau_log                                0x0001101c   Data          16  tau_log.o(.ARM.__at_0x1101C)
    sg_pq_para                               0x0001102c   Data          22  hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C)
    MIPI_RX_IRQn_Handler                     0x00011045   Thumb Code   354  drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler)
    UART_IRQn_Handler                        0x000113a9   Thumb Code   364  drv_uart.o(i.UART_IRQn_Handler)
    __0vsprintf                              0x00011529   Thumb Code    30  printfa.o(i.__0vsprintf)
    __1vsprintf                              0x00011529   Thumb Code     0  printfa.o(i.__0vsprintf)
    __2vsprintf                              0x00011529   Thumb Code     0  printfa.o(i.__0vsprintf)
    __c89vsprintf                            0x00011529   Thumb Code     0  printfa.o(i.__0vsprintf)
    vsprintf                                 0x00011529   Thumb Code     0  printfa.o(i.__0vsprintf)
    __ARM_clz                                0x0001154d   Thumb Code    46  depilogue.o(i.__ARM_clz)
    __ARM_common_switch8                     0x0001157b   Thumb Code    26  hal_dsi_rx_ctrl.o(i.__ARM_common_switch8)
    __scatterload_copy                       0x000115cd   Thumb Code    14  handlers.o(i.__scatterload_copy)
    __scatterload_zeroinit                   0x000115db   Thumb Code    14  handlers.o(i.__scatterload_zeroinit)
    app_display_init                         0x000121b9   Thumb Code    58  s8_demo.o(i.app_display_init)
    app_gpio_init                            0x00012221   Thumb Code    28  s8_demo.o(i.app_gpio_init)
    board_Init                               0x000126e1   Thumb Code    38  board.o(i.board_Init)
    ceil                                     0x0001270d   Thumb Code   180  ceil.o(i.ceil)
    dcs_packet_fifo_alloc                    0x00012889   Thumb Code    80  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    dcs_packet_fifo_init                     0x000128e1   Thumb Code    18  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    dcs_packet_free_fifo_header              0x000128f9   Thumb Code    60  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    dcs_packet_get_fifo_header               0x0001293d   Thumb Code    26  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    delayMs                                  0x00012961   Thumb Code    24  tau_delay.o(i.delayMs)
    delayUs                                  0x00012979   Thumb Code    40  tau_delay.o(i.delayUs)
    drv_common_system_init                   0x000129a5   Thumb Code     8  drv_common.o(i.drv_common_system_init)
    drv_crgu_enable_clock                    0x000129ad   Thumb Code    54  drv_crgu.o(i.drv_crgu_enable_clock)
    drv_crgu_get_rxbr_clk                    0x000129e9   Thumb Code    70  drv_crgu.o(i.drv_crgu_get_rxbr_clk)
    drv_crgu_reset_modules                   0x00012a51   Thumb Code    10  drv_crgu.o(i.drv_crgu_reset_modules)
    drv_crgu_set_ahb_clk                     0x00012a61   Thumb Code    34  drv_crgu.o(i.drv_crgu_set_ahb_clk)
    drv_crgu_set_clock_div                   0x00012a89   Thumb Code    12  drv_crgu.o(i.drv_crgu_set_clock_div)
    drv_crgu_set_dpi_clk                     0x00012a99   Thumb Code    54  drv_crgu.o(i.drv_crgu_set_dpi_clk)
    drv_crgu_set_dsc_clk                     0x00012ad5   Thumb Code    52  drv_crgu.o(i.drv_crgu_set_dsc_clk)
    drv_crgu_set_fb_clk                      0x00012b0d   Thumb Code    34  drv_crgu.o(i.drv_crgu_set_fb_clk)
    drv_crgu_set_lcdc_clk                    0x00012b35   Thumb Code    36  drv_crgu.o(i.drv_crgu_set_lcdc_clk)
    drv_crgu_set_reset                       0x00012b5d   Thumb Code    20  drv_crgu.o(i.drv_crgu_set_reset)
    drv_crgu_set_rxbr_clk                    0x00012b75   Thumb Code    34  drv_crgu.o(i.drv_crgu_set_rxbr_clk)
    drv_crgu_set_vidc_clk                    0x00012b9d   Thumb Code    36  drv_crgu.o(i.drv_crgu_set_vidc_clk)
    drv_dma_clear_status                     0x00012bc5   Thumb Code    20  drv_dma.o(i.drv_dma_clear_status)
    drv_dsc_dec_disable                      0x00012bf1   Thumb Code    20  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    drv_dsc_dec_enable                       0x00012c0d   Thumb Code    44  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    drv_dsc_dec_get_nslc                     0x00012c49   Thumb Code    22  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    drv_dsi_rx_calc_ipi_tx_delay             0x00012c69   Thumb Code   252  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    drv_dsi_rx_enable_irq                    0x00012d75   Thumb Code    58  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    drv_dsi_rx_get_compression_en            0x00012e21   Thumb Code    10  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    drv_dsi_rx_get_ddi_crc_en                0x00012e31   Thumb Code    10  drv_dsi_rx.o(i.drv_dsi_rx_get_ddi_crc_en)
    drv_dsi_rx_power_up                      0x00012e41   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    drv_dsi_rx_set_check_crc                 0x00012e59   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc)
    drv_dsi_rx_set_ctrl_cfg                  0x00012e75   Thumb Code    32  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    drv_dsi_rx_set_ddi_cfg                   0x00012e99   Thumb Code    10  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    drv_dsi_rx_set_ddi_crc_en                0x00012ea9   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_crc_en)
    drv_dsi_rx_set_inten                     0x00012ec5   Thumb Code     8  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    drv_dsi_rx_set_ipi_cfg                   0x00012ed1   Thumb Code    12  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    drv_dsi_rx_set_ipi_ycbcr_frmt            0x00012ee1   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_ycbcr_frmt)
    drv_dsi_rx_set_lane_swap                 0x00012efd   Thumb Code    16  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    drv_dsi_rx_set_resp_cnt                  0x00012f11   Thumb Code    32  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    drv_dsi_rx_set_tear_resp_en              0x00012f35   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_tear_resp_en)
    drv_dsi_rx_set_up_phy                    0x00012f51   Thumb Code   136  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    drv_dsi_rx_shut_down                     0x00012fe9   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    drv_dsi_tx_command_header                0x00013001   Thumb Code    18  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    drv_dsi_tx_command_mode_cfg              0x00013019   Thumb Code    82  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    drv_dsi_tx_command_put_payload           0x00013071   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    drv_dsi_tx_config_eotp                   0x0001307d   Thumb Code    26  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    drv_dsi_tx_config_int                    0x0001309d   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    drv_dsi_tx_dpi_lpcmd_time                0x000130a9   Thumb Code    10  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    drv_dsi_tx_dpi_mode                      0x000130b9   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    drv_dsi_tx_dpi_polarity                  0x000130c9   Thumb Code    32  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    drv_dsi_tx_edpi_cmd_size                 0x000130ed   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    drv_dsi_tx_get_cmd_status                0x000130f9   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    drv_dsi_tx_mode                          0x00013105   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    drv_dsi_tx_phy_clock_lane_auto_lp        0x00013111   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    drv_dsi_tx_phy_clock_lane_req_hs         0x0001312d   Thumb Code    26  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    drv_dsi_tx_phy_lane_mode                 0x0001314d   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    drv_dsi_tx_phy_status_ready              0x0001315d   Thumb Code   100  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    drv_dsi_tx_phy_status_stopstate          0x000131c5   Thumb Code    62  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    drv_dsi_tx_phy_test_setup                0x00013209   Thumb Code   314  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    drv_dsi_tx_phy_time_cfg                  0x00013359   Thumb Code    28  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    drv_dsi_tx_powerup                       0x00013379   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    drv_dsi_tx_response_mode                 0x00013385   Thumb Code    30  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    drv_dsi_tx_set_bta_ack                   0x000133a9   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    drv_dsi_tx_set_esc_div                   0x000133c5   Thumb Code    14  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    drv_dsi_tx_set_int                       0x000133d9   Thumb Code    58  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    drv_dsi_tx_set_time_out_div              0x00013419   Thumb Code    18  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    drv_dsi_tx_set_video_chunk               0x00013431   Thumb Code    14  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    drv_dsi_tx_set_video_timing              0x00013445   Thumb Code    30  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    drv_dsi_tx_shutdown                      0x00013469   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    drv_dsi_tx_timeout_cfg                   0x00013475   Thumb Code    38  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    drv_dsi_tx_video_mode_cfg                0x000134a1   Thumb Code   226  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    drv_efuse_enter_inactive                 0x00013589   Thumb Code    54  drv_efuse.o(i.drv_efuse_enter_inactive)
    drv_efuse_int_enable                     0x000135bf   Thumb Code    12  drv_efuse.o(i.drv_efuse_int_enable)
    drv_efuse_read                           0x000135cb   Thumb Code    58  drv_efuse.o(i.drv_efuse_read)
    drv_efuse_read_req                       0x00013605   Thumb Code    24  drv_efuse.o(i.drv_efuse_read_req)
    drv_gpio_get_attribute                   0x0001361d   Thumb Code    12  drv_gpio.o(i.drv_gpio_get_attribute)
    drv_gpio_register_ap_reset_callback      0x00013651   Thumb Code     6  drv_gpio.o(i.drv_gpio_register_ap_reset_callback)
    drv_gpio_register_callback               0x0001365d   Thumb Code    14  drv_gpio.o(i.drv_gpio_register_callback)
    drv_gpio_set_attribute                   0x00013671   Thumb Code    22  drv_gpio.o(i.drv_gpio_set_attribute)
    drv_gpio_set_int                         0x0001368d   Thumb Code    62  drv_gpio.o(i.drv_gpio_set_int)
    drv_gpio_set_ioe                         0x000136d1   Thumb Code    26  drv_gpio.o(i.drv_gpio_set_ioe)
    drv_gpio_set_mode                        0x000136f1   Thumb Code    16  drv_gpio.o(i.drv_gpio_set_mode)
    drv_lcdc_bcsa_config                     0x00013725   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_bcsa_config)
    drv_lcdc_cfg_int_frame                   0x0001374d   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_cfg_int_frame)
    drv_lcdc_cmd_start                       0x00013791   Thumb Code    46  drv_lcdc.o(i.drv_lcdc_cmd_start)
    drv_lcdc_config_acc_command_mode         0x000137c5   Thumb Code    14  drv_lcdc.o(i.drv_lcdc_config_acc_command_mode)
    drv_lcdc_config_int                      0x000137d9   Thumb Code    50  drv_lcdc.o(i.drv_lcdc_config_int)
    drv_lcdc_config_int_single               0x00013811   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_int_single)
    drv_lcdc_config_overwrite_rgb            0x00013839   Thumb Code    18  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    drv_lcdc_config_src_parameter            0x00013851   Thumb Code    72  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    drv_lcdc_crop_hact                       0x000138a1   Thumb Code    10  drv_lcdc.o(i.drv_lcdc_crop_hact)
    drv_lcdc_ctrl_flow                       0x000138b1   Thumb Code    50  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    drv_lcdc_dith_config                     0x000138e9   Thumb Code    40  drv_lcdc.o(i.drv_lcdc_dith_config)
    drv_lcdc_edge_dect_config                0x00013919   Thumb Code    50  drv_lcdc.o(i.drv_lcdc_edge_dect_config)
    drv_lcdc_edge_enh_config                 0x00013955   Thumb Code    86  drv_lcdc.o(i.drv_lcdc_edge_enh_config)
    drv_lcdc_enable_shadow_reg               0x000139b9   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    drv_lcdc_endianness_config               0x000139dd   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_endianness_config)
    drv_lcdc_fc_config                       0x000139f9   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_fc_config)
    drv_lcdc_fldc_config                     0x00013a19   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_fldc_config)
    drv_lcdc_function_disable                0x00013a3d   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_function_disable)
    drv_lcdc_function_enable                 0x00013a61   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_function_enable)
    drv_lcdc_set_int                         0x00013a85   Thumb Code    54  drv_lcdc.o(i.drv_lcdc_set_int)
    drv_lcdc_set_prefetch                    0x00013ac1   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_set_prefetch)
    drv_lcdc_set_tear_line                   0x00013add   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_set_tear_line)
    drv_lcdc_stop_display                    0x00013af9   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_stop_display)
    drv_lcdc_vid_hw_start                    0x00013b09   Thumb Code    56  drv_lcdc.o(i.drv_lcdc_vid_hw_start)
    drv_lcdc_vintp_mode_config               0x00013b45   Thumb Code    18  drv_lcdc.o(i.drv_lcdc_vintp_mode_config)
    drv_memc_clear_status                    0x00013b5d   Thumb Code    14  drv_memc.o(i.drv_memc_clear_status)
    drv_memc_enable_irq                      0x00013b71   Thumb Code    58  drv_memc.o(i.drv_memc_enable_irq)
    drv_memc_gen_a_tear_signal               0x00013bb1   Thumb Code    12  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    drv_memc_get_status                      0x00013bc1   Thumb Code    20  drv_memc.o(i.drv_memc_get_status)
    drv_memc_get_tear_mode                   0x00013bd9   Thumb Code    10  drv_memc.o(i.drv_memc_get_tear_mode)
    drv_memc_rate_transfer_sel               0x00013be9   Thumb Code    22  drv_memc.o(i.drv_memc_rate_transfer_sel)
    drv_memc_sel_vsync                       0x00013c05   Thumb Code    16  drv_memc.o(i.drv_memc_sel_vsync)
    drv_memc_set_active_height               0x00013c19   Thumb Code    16  drv_memc.o(i.drv_memc_set_active_height)
    drv_memc_set_circ_mode_enable            0x00013c31   Thumb Code    24  drv_memc.o(i.drv_memc_set_circ_mode_enable)
    drv_memc_set_data_mode                   0x00013c4d   Thumb Code    14  drv_memc.o(i.drv_memc_set_data_mode)
    drv_memc_set_double_buffer               0x00013c61   Thumb Code    18  drv_memc.o(i.drv_memc_set_double_buffer)
    drv_memc_set_frame_drop_select           0x00013c79   Thumb Code    24  drv_memc.o(i.drv_memc_set_frame_drop_select)
    drv_memc_set_fs_en_conditions            0x00013c95   Thumb Code    18  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    drv_memc_set_lcdc_st_conditions          0x00013cad   Thumb Code    20  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    drv_memc_set_ltpo_mode                   0x00013cc9   Thumb Code    28  drv_memc.o(i.drv_memc_set_ltpo_mode)
    drv_memc_set_ltpo_pu_thres               0x00013ce9   Thumb Code    18  drv_memc.o(i.drv_memc_set_ltpo_pu_thres)
    drv_memc_set_tear_mode                   0x00013d01   Thumb Code    16  drv_memc.o(i.drv_memc_set_tear_mode)
    drv_memc_set_tear_waveform               0x00013d15   Thumb Code    36  drv_memc.o(i.drv_memc_set_tear_waveform)
    drv_memc_set_vidc_sync_cnt               0x00013d41   Thumb Code    16  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    drv_phy_test_clear                       0x00013d55   Thumb Code    16  drv_phy_common.o(i.drv_phy_test_clear)
    drv_phy_test_lock                        0x00013d65   Thumb Code    24  drv_phy_common.o(i.drv_phy_test_lock)
    drv_pwr_efuse_pd                         0x00013d7d   Thumb Code    36  drv_pwr.o(i.drv_pwr_efuse_pd)
    drv_pwr_enter_deep_sleep_mode            0x00013dad   Thumb Code    50  drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode)
    drv_pwr_enter_sleep_mode_ex              0x00013ded   Thumb Code    26  drv_pwr.o(i.drv_pwr_enter_sleep_mode_ex)
    drv_pwr_enter_stop_sleep_mode            0x00013e15   Thumb Code   124  drv_pwr.o(i.drv_pwr_enter_stop_sleep_mode)
    drv_pwr_exit_sleep_mode                  0x00013ea1   Thumb Code    32  drv_pwr.o(i.drv_pwr_exit_sleep_mode)
    drv_pwr_get_power_ready_st               0x00013ec9   Thumb Code    10  drv_pwr.o(i.drv_pwr_get_power_ready_st)
    drv_pwr_set_breath_screen_power_sel      0x00013ed9   Thumb Code    34  drv_pwr.o(i.drv_pwr_set_breath_screen_power_sel)
    drv_pwr_set_digit_power_sel              0x00013f01   Thumb Code    34  drv_pwr.o(i.drv_pwr_set_digit_power_sel)
    drv_pwr_set_pll_clk                      0x00013f29   Thumb Code    30  drv_pwr.o(i.drv_pwr_set_pll_clk)
    drv_pwr_set_wakeup_type                  0x00013f5d   Thumb Code    40  drv_pwr.o(i.drv_pwr_set_wakeup_type)
    drv_pwr_write_lock                       0x00013f89   Thumb Code    18  drv_pwr.o(i.drv_pwr_write_lock)
    drv_rxbr_clear_pkt_buffer                0x00013fa9   Thumb Code    12  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    drv_rxbr_clear_status0                   0x00013fb9   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_clear_status0)
    drv_rxbr_enable_irq                      0x00013fc5   Thumb Code    90  drv_rxbr.o(i.drv_rxbr_enable_irq)
    drv_rxbr_frame_drop_cfg                  0x00014021   Thumb Code    18  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    drv_rxbr_hline_rcv1_cfg                  0x0001406d   Thumb Code    14  drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg)
    drv_rxbr_hline_rcv_cfg                   0x00014081   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    drv_rxbr_register_irq1_callback          0x00014091   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    drv_rxbr_set_cmd_response                0x0001409d   Thumb Code   320  drv_rxbr.o(i.drv_rxbr_set_cmd_response)
    drv_rxbr_set_color_format                0x000141e1   Thumb Code    24  drv_rxbr.o(i.drv_rxbr_set_color_format)
    drv_rxbr_set_filter_regs                 0x000141fd   Thumb Code    32  drv_rxbr.o(i.drv_rxbr_set_filter_regs)
    drv_rxbr_set_inten                       0x00014221   Thumb Code    22  drv_rxbr.o(i.drv_rxbr_set_inten)
    drv_rxbr_set_ltpo_drop_th                0x0001423d   Thumb Code    18  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    drv_rxbr_set_usr_cfg                     0x00014255   Thumb Code    56  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    drv_rxbr_set_usr_col                     0x00014295   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    drv_rxbr_set_usr_row                     0x000142a5   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    drv_se_init                              0x000142b5   Thumb Code   106  drv_se.o(i.drv_se_init)
    drv_se_set_dsc                           0x0001432d   Thumb Code   162  drv_se.o(i.drv_se_set_dsc)
    drv_se_set_lcdc                          0x00014401   Thumb Code    88  drv_se.o(i.drv_se_set_lcdc)
    drv_se_set_memc                          0x00014489   Thumb Code    96  drv_se.o(i.drv_se_set_memc)
    drv_se_set_rxbr                          0x00014519   Thumb Code   158  drv_se.o(i.drv_se_set_rxbr)
    drv_se_set_vidc                          0x000145e9   Thumb Code   122  drv_se.o(i.drv_se_set_vidc)
    drv_se_start_rx                          0x00014695   Thumb Code    16  drv_se.o(i.drv_se_start_rx)
    drv_spim_clear_int_status                0x000146a9   Thumb Code     8  drv_spi_master.o(i.drv_spim_clear_int_status)
    drv_spim_disable_int                     0x000146b5   Thumb Code    38  drv_spi_master.o(i.drv_spim_disable_int)
    drv_spim_get_busy                        0x000146e5   Thumb Code    10  drv_spi_master.o(i.drv_spim_get_busy)
    drv_spim_get_int_status                  0x000146f5   Thumb Code     6  drv_spi_master.o(i.drv_spim_get_int_status)
    drv_spim_set_inten                       0x00014701   Thumb Code    22  drv_spi_master.o(i.drv_spim_set_inten)
    drv_swire_enable                         0x0001471d   Thumb Code    24  drv_swire.o(i.drv_swire_enable)
    drv_swire_get_pulse_count                0x00014739   Thumb Code     6  drv_swire.o(i.drv_swire_get_pulse_count)
    drv_swire_register_callback              0x00014745   Thumb Code     6  drv_swire.o(i.drv_swire_register_callback)
    drv_swire_set_bit_time                   0x00014751   Thumb Code    18  drv_swire.o(i.drv_swire_set_bit_time)
    drv_swire_set_int                        0x00014769   Thumb Code    64  drv_swire.o(i.drv_swire_set_int)
    drv_swire_set_power_down                 0x000147b1   Thumb Code    24  drv_swire.o(i.drv_swire_set_power_down)
    drv_swire_set_pulse_count                0x000147cd   Thumb Code     6  drv_swire.o(i.drv_swire_set_pulse_count)
    drv_swire_set_trig_mode                  0x000147d9   Thumb Code    24  drv_swire.o(i.drv_swire_set_trig_mode)
    drv_sys_cfg_clear_all_int                0x000147f5   Thumb Code     8  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    drv_sys_cfg_clear_pending                0x00014801   Thumb Code    32  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    drv_sys_cfg_sel_ap_rst_trig              0x00014829   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig)
    drv_sys_cfg_sel_gpio_group               0x0001484d   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group)
    drv_sys_cfg_sel_int_trig                 0x00014871   Thumb Code    32  drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig)
    drv_sys_cfg_sel_swire_timer              0x00014895   Thumb Code    18  drv_sys_cfg.o(i.drv_sys_cfg_sel_swire_timer)
    drv_sys_cfg_set_int                      0x000148ad   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    drv_timer_enable                         0x000148eb   Thumb Code    32  drv_timer.o(i.drv_timer_enable)
    drv_timer_get_instance                   0x0001490d   Thumb Code    10  drv_timer.o(i.drv_timer_get_instance)
    drv_timer_register_callback              0x00014959   Thumb Code    14  drv_timer.o(i.drv_timer_register_callback)
    drv_timer_set_compare_val                0x0001496d   Thumb Code    50  drv_timer.o(i.drv_timer_set_compare_val)
    drv_timer_set_int                        0x000149ad   Thumb Code    68  drv_timer.o(i.drv_timer_set_int)
    drv_timer_set_prescaler                  0x000149f5   Thumb Code    36  drv_timer.o(i.drv_timer_set_prescaler)
    drv_timer_set_repeat                     0x00014a1d   Thumb Code    12  drv_timer.o(i.drv_timer_set_repeat)
    drv_tx_phy_test_enter                    0x00014a2d   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    drv_tx_phy_test_exit                     0x00014a4d   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    drv_tx_phy_test_write_code               0x00014a6d   Thumb Code    34  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    drv_uart_abort_recv                      0x00014a95   Thumb Code    46  drv_uart.o(i.drv_uart_abort_recv)
    drv_uart_abort_send                      0x00014ac9   Thumb Code    46  drv_uart.o(i.drv_uart_abort_send)
    drv_uart_config_int                      0x00014afd   Thumb Code    20  drv_uart.o(i.drv_uart_config_int)
    drv_uart_enable_int                      0x00014b29   Thumb Code    84  drv_uart.o(i.drv_uart_enable_int)
    drv_uart_get_instance                    0x00014b85   Thumb Code    36  drv_uart.o(i.drv_uart_get_instance)
    drv_uart_init                            0x00014bad   Thumb Code   206  drv_uart.o(i.drv_uart_init)
    drv_uart_reset_rx_fifo                   0x00014cb9   Thumb Code    28  drv_uart.o(i.drv_uart_reset_rx_fifo)
    drv_uart_reset_tx_fifo                   0x00014cd5   Thumb Code    28  drv_uart.o(i.drv_uart_reset_tx_fifo)
    drv_uart_send_blocking                   0x00014cf1   Thumb Code    26  drv_uart.o(i.drv_uart_send_blocking)
    drv_uart_set_baud_rate                   0x00014d0b   Thumb Code    84  drv_uart.o(i.drv_uart_set_baud_rate)
    drv_uart_trans_create_handle             0x00014d61   Thumb Code    72  drv_uart.o(i.drv_uart_trans_create_handle)
    drv_vidc_clear_irq                       0x00014dad   Thumb Code    10  drv_vidc.o(i.drv_vidc_clear_irq)
    drv_vidc_enable                          0x00014dbd   Thumb Code    26  drv_vidc.o(i.drv_vidc_enable)
    drv_vidc_enable_irq                      0x00014ddd   Thumb Code    58  drv_vidc.o(i.drv_vidc_enable_irq)
    drv_vidc_get_int_source                  0x00014e1d   Thumb Code    40  drv_vidc.o(i.drv_vidc_get_int_source)
    drv_vidc_get_irq_status                  0x00014e49   Thumb Code    20  drv_vidc.o(i.drv_vidc_get_irq_status)
    drv_vidc_init_module_enable              0x00014e61   Thumb Code    36  drv_vidc.o(i.drv_vidc_init_module_enable)
    drv_vidc_register_callback               0x00014e8d   Thumb Code     6  drv_vidc.o(i.drv_vidc_register_callback)
    drv_vidc_reset                           0x00014e99   Thumb Code     8  drv_vidc.o(i.drv_vidc_reset)
    drv_vidc_set_circ_mode_enable            0x00014ea5   Thumb Code    24  drv_vidc.o(i.drv_vidc_set_circ_mode_enable)
    drv_vidc_set_dither_config               0x00014ec1   Thumb Code    50  drv_vidc.o(i.drv_vidc_set_dither_config)
    drv_vidc_set_dst_parameter               0x00014ef9   Thumb Code    86  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    drv_vidc_set_honly_hcoef0                0x00014f55   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_honly_hcoef0)
    drv_vidc_set_honly_hinitb                0x00014f61   Thumb Code    38  drv_vidc.o(i.drv_vidc_set_honly_hinitb)
    drv_vidc_set_honly_hinitr                0x00014f8d   Thumb Code    42  drv_vidc.o(i.drv_vidc_set_honly_hinitr)
    drv_vidc_set_irqen                       0x00014fbd   Thumb Code    22  drv_vidc.o(i.drv_vidc_set_irqen)
    drv_vidc_set_mirror                      0x00014fd9   Thumb Code    16  drv_vidc.o(i.drv_vidc_set_mirror)
    drv_vidc_set_pentile_swap                0x00014fed   Thumb Code    20  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    drv_vidc_set_pu_ctrl                     0x00015009   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    drv_vidc_set_rotation                    0x00015015   Thumb Code    18  drv_vidc.o(i.drv_vidc_set_rotation)
    drv_vidc_set_scld_hcoef0                 0x0001502d   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    drv_vidc_set_scld_hcoef1                 0x00015039   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    drv_vidc_set_scld_step                   0x00015045   Thumb Code    14  drv_vidc.o(i.drv_vidc_set_scld_step)
    drv_vidc_set_scld_vcoef0                 0x00015059   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    drv_vidc_set_scld_vcoef1                 0x00015065   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    drv_vidc_set_src_parameter               0x00015071   Thumb Code    28  drv_vidc.o(i.drv_vidc_set_src_parameter)
    drv_vidc_set_vintp_config                0x00015091   Thumb Code    52  drv_vidc.o(i.drv_vidc_set_vintp_config)
    drv_wdg_clear_counter                    0x000150c9   Thumb Code    12  drv_wdg.o(i.drv_wdg_clear_counter)
    drv_wdg_set_int                          0x000150f9   Thumb Code    48  drv_wdg.o(i.drv_wdg_set_int)
    fputc                                    0x0001512d   Thumb Code    42  tau_log.o(i.fputc)
    hal_dsi_rx_ctrl_create_handle            0x000151a1   Thumb Code    52  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    hal_dsi_rx_ctrl_dcs_async_handler        0x000151d9   Thumb Code    60  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler)
    hal_dsi_rx_ctrl_deinit                   0x00015219   Thumb Code   132  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit)
    hal_dsi_rx_ctrl_init                     0x000152ad   Thumb Code   136  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    hal_dsi_rx_ctrl_pre_init_pps             0x000159e1   Thumb Code    50  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    hal_dsi_rx_ctrl_set_auto_ack             0x00015a19   Thumb Code   148  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack)
    hal_dsi_rx_ctrl_start                    0x00015af9   Thumb Code    42  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    hal_dsi_rx_ctrl_stop                     0x00015b29   Thumb Code    42  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop)
    hal_dsi_rx_ctrl_toggle_resolution        0x00015b59   Thumb Code    28  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    hal_dsi_tx_ctrl_create_handle            0x00015df5   Thumb Code    48  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    hal_dsi_tx_ctrl_deinit                   0x00015e2d   Thumb Code    84  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit)
    hal_dsi_tx_ctrl_gen_a_tear_signal        0x00015e8d   Thumb Code    34  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal)
    hal_dsi_tx_ctrl_init                     0x00015eb1   Thumb Code   108  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    hal_dsi_tx_ctrl_set_overwrite_rgb        0x00015f35   Thumb Code     8  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    hal_dsi_tx_ctrl_set_tear_mode            0x00015f3d   Thumb Code    10  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode)
    hal_dsi_tx_ctrl_start                    0x00015f49   Thumb Code   108  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    hal_dsi_tx_ctrl_stop                     0x00015fb9   Thumb Code    52  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop)
    hal_dsi_tx_ctrl_write_array_cmd          0x00015ff1   Thumb Code   238  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd)
    hal_dsi_tx_ctrl_write_cmd                0x000160e5   Thumb Code   202  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    hal_gpio_config_pad                      0x00016781   Thumb Code    58  hal_gpio.o(i.hal_gpio_config_pad)
    hal_gpio_ctrl_eint                       0x000167bd   Thumb Code    20  hal_gpio.o(i.hal_gpio_ctrl_eint)
    hal_gpio_init_eint                       0x000167d5   Thumb Code    60  hal_gpio.o(i.hal_gpio_init_eint)
    hal_gpio_init_input                      0x00016815   Thumb Code    30  hal_gpio.o(i.hal_gpio_init_input)
    hal_gpio_init_output                     0x00016839   Thumb Code    36  hal_gpio.o(i.hal_gpio_init_output)
    hal_gpio_reg_eint_cb                     0x00016861   Thumb Code    20  hal_gpio.o(i.hal_gpio_reg_eint_cb)
    hal_gpio_set_ap_reset_int                0x00016879   Thumb Code    76  hal_gpio.o(i.hal_gpio_set_ap_reset_int)
    hal_gpio_set_mode                        0x000168c9   Thumb Code    96  hal_gpio.o(i.hal_gpio_set_mode)
    hal_gpio_set_output_data                 0x0001692d   Thumb Code     8  hal_gpio.o(i.hal_gpio_set_output_data)
    hal_gpio_set_pull_state                  0x00016935   Thumb Code    66  hal_gpio.o(i.hal_gpio_set_pull_state)
    hal_internal_sync_get_hight_performan_mode 0x0001697d   Thumb Code    10  hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode)
    hal_internal_sync_input_resolution_change 0x0001698d   Thumb Code   326  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    hal_internal_sync_register_lcdc_cb       0x00016b3d   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb)
    hal_internal_vsync_deinit                0x00016b49   Thumb Code    22  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    hal_internal_vsync_get_rx_state          0x00016b69   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state)
    hal_internal_vsync_get_sync_line         0x00016b75   Thumb Code    18  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    hal_internal_vsync_get_tx_state          0x00016b8d   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    hal_internal_vsync_init_rx               0x00016b99   Thumb Code   190  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    hal_internal_vsync_init_tx               0x00016c71   Thumb Code   190  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    hal_internal_vsync_set_rx_state          0x00016d35   Thumb Code    28  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    hal_internal_vsync_set_tear_mode         0x00016d55   Thumb Code   230  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    hal_internal_vsync_set_tx_state          0x00016e4d   Thumb Code    92  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    hal_intl_dcs_init_sw_fltr                0x00016eb9   Thumb Code    90  hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr)
    hal_intl_dcs_set_auto_hw_filter          0x0001756d   Thumb Code   130  hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter)
    hal_intl_fb_cal_fb_info                  0x00017625   Thumb Code   724  hal_internal_fb.o(i.hal_intl_fb_cal_fb_info)
    hal_intl_fb_get_memc_flow_mode           0x00017a95   Thumb Code     6  hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode)
    hal_intl_fb_get_rx_fb_info               0x00017aa1   Thumb Code    12  hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info)
    hal_intl_fb_get_tx_fb_info               0x00017ab1   Thumb Code    12  hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info)
    hal_intl_fb_get_user_flow                0x00017ac1   Thumb Code     6  hal_internal_fb.o(i.hal_intl_fb_get_user_flow)
    hal_intl_svs_deinit_rx                   0x00017acd   Thumb Code    32  hal_internal_svs.o(i.hal_intl_svs_deinit_rx)
    hal_intl_svs_deinit_tx                   0x00017af5   Thumb Code    10  hal_internal_svs.o(i.hal_intl_svs_deinit_tx)
    hal_intl_svs_handle                      0x00017b05   Thumb Code    24  hal_internal_svs.o(i.hal_intl_svs_handle)
    hal_intl_svs_init_rx                     0x00017b29   Thumb Code   120  hal_internal_svs.o(i.hal_intl_svs_init_rx)
    hal_intl_svs_init_tx                     0x00017ba9   Thumb Code    16  hal_internal_svs.o(i.hal_intl_svs_init_tx)
    hal_intl_svs_set_rx_vtt                  0x00017bbd   Thumb Code     6  hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt)
    hal_intl_svs_update_rxbr_clk             0x00017bc9   Thumb Code    52  hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk)
    hal_lcdc_displayproc_config              0x00017c11   Thumb Code    94  hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config)
    hal_lcdc_func_update                     0x00017c81   Thumb Code    90  hal_dsi_tx_ctrl.o(i.hal_lcdc_func_update)
    hal_lcdc_postproc_config                 0x00017d95   Thumb Code   276  hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config)
    hal_lcdc_upscaler_config                 0x00017f1d   Thumb Code   190  hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config)
    hal_pwr_enter_deep_sleep_mode            0x00017ff1   Thumb Code    42  hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode)
    hal_pwr_enter_normal_sleep_mode          0x0001801b   Thumb Code     8  hal_pwr.o(i.hal_pwr_enter_normal_sleep_mode)
    hal_pwr_enter_stop_sleep_mode            0x00018025   Thumb Code    88  hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode)
    hal_pwr_exit_sleep_mode                  0x00018089   Thumb Code    10  hal_pwr.o(i.hal_pwr_exit_sleep_mode)
    hal_pwr_get_vcc_power_ready              0x00018093   Thumb Code     8  hal_pwr.o(i.hal_pwr_get_vcc_power_ready)
    hal_pwr_set_main_power                   0x0001809b   Thumb Code     8  hal_pwr.o(i.hal_pwr_set_main_power)
    hal_pwr_set_sleep_mode_power             0x000180a3   Thumb Code     8  hal_pwr.o(i.hal_pwr_set_sleep_mode_power)
    hal_pwr_set_stop_sleep_wakeup_pin        0x000180ad   Thumb Code    86  hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin)
    hal_swire_deinit                         0x00018111   Thumb Code    60  hal_swire.o(i.hal_swire_deinit)
    hal_swire_enable                         0x00018151   Thumb Code    86  hal_swire.o(i.hal_swire_enable)
    hal_swire_init                           0x000181ad   Thumb Code    74  hal_swire.o(i.hal_swire_init)
    hal_swire_set_pulse                      0x00018205   Thumb Code    32  hal_swire.o(i.hal_swire_set_pulse)
    hal_swire_set_timer                      0x00018229   Thumb Code    60  hal_swire.o(i.hal_swire_set_timer)
    hal_system_init                          0x00018269   Thumb Code   224  hal_system.o(i.hal_system_init)
    hal_timer_deinit                         0x00018381   Thumb Code    48  hal_timer.o(i.hal_timer_deinit)
    hal_timer_init                           0x000183b1   Thumb Code    28  hal_timer.o(i.hal_timer_init)
    hal_timer_set_repeat                     0x000183cd   Thumb Code     8  hal_timer.o(i.hal_timer_set_repeat)
    hal_timer_start                          0x000183d5   Thumb Code    48  hal_timer.o(i.hal_timer_start)
    hal_timer_stop                           0x00018405   Thumb Code    40  hal_timer.o(i.hal_timer_stop)
    hal_uart_init                            0x0001845d   Thumb Code   134  hal_uart.o(i.hal_uart_init)
    hal_uart_send_blocking                   0x000184f1   Thumb Code    24  hal_uart.o(i.hal_uart_send_blocking)
    hal_vsync_reset_lcdc_scaler              0x0001850d   Thumb Code   188  hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler)
    main                                     0x000185d9   Thumb Code    32  main.o(i.main)
    s8_demo                                  0x00018919   Thumb Code    48  s8_demo.o(i.s8_demo)
    tau_log_init                             0x00018ea9   Thumb Code    48  tau_log.o(i.tau_log_init)
    tau_log_printf                           0x00018edd   Thumb Code   116  tau_log.o(i.tau_log_printf)
    tau_log_push_log                         0x00018f61   Thumb Code   118  tau_log.o(i.tau_log_push_log)
    panel_init_code                          0x0001921c   Data        7815  s8_demo.o(.constdata)
    Region$$Table$$Base                      0x0001b3b4   Number         0  anon$$obj.o(Region$$Table)
    Region$$Table$$Limit                     0x0001b3d4   Number         0  anon$$obj.o(Region$$Table)
    s_swire_pwm_counter                      0x0007000d   Data           1  s8_demo.o(.data)
    t_pps                                    0x0007000e   Data         128  s8_demo.o(.data)
    sg_uart0_tx_handle                       0x00070104   Data           4  hal_uart.o(.data)
    sg_uart0_rx_handle                       0x00070108   Data           4  hal_uart.o(.data)
    sg_uart1_tx_handle                       0x0007010c   Data           4  hal_uart.o(.data)
    sg_uart1_rx_handle                       0x00070110   Data           4  hal_uart.o(.data)
    g_sof_gen_te_func                        0x0007011c   Data           4  hal_internal_vsync.o(.data)
    hal_internal_lcdc_handle_callback        0x00070120   Data           4  hal_internal_vsync.o(.data)
    g_systick_cb_func                        0x0007014c   Data           4  drv_common.o(.data)
    g_system_clock                           0x00070150   Data           4  drv_common.o(.data)
    g_system_delay_step                      0x00070154   Data           1  drv_common.o(.data)
    cuckoo_dma_req_map                       0x00070258   Data         144  drv_dma.o(.data)
    drv_i2c_table                            0x0007034c   Data          60  drv_i2c.o(.data)
    g_int_rxbr_irq0_cb_func                  0x00070390   Data           4  drv_rxbr.o(.data)
    g_int_rxbr_irq1_cb_func                  0x00070394   Data           4  drv_rxbr.o(.data)
    g_int_vidc_cb_func                       0x00070398   Data           4  drv_vidc.o(.data)
    __stdout                                 0x0007039c   Data           4  stdout.o(.data)
    g_vsync_handle                           0x00070620   Data          36  hal_internal_vsync.o(.bss)
    g_dcs_execute_table                      0x00070644   Data        2048  hal_internal_dcs.o(.bss)
    g_rx_fb_info                             0x00070f44   Data          68  hal_internal_fb.o(.bss)
    g_packet_fifo                            0x0007101c   Data        4204  dcs_packet_fifo.o(.bss)
    __stack_limit                            0x000720e8   Data           0  startup_armcm0.o(STACK)
    __initial_sp                             0x000730e8   Data           0  startup_armcm0.o(STACK)



==============================================================================

Memory Map of the image

  Image Entry point : 0x000100c1

  Load Region LR_IROM2 (Base: 0x00010000, Size: 0x0000b774, Max: 0x00010000, ABSOLUTE, COMPRESSED[0x0000b538])

    Execution Region ER_IROM2 (Exec base: 0x00010000, Load base: 0x00010000, Size: 0x0000b3d4, Max: 0x00010000, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00010000   0x00010000   0x000000c0   Data   RO          538    RESET               startup_armcm0.o
    0x000100c0   0x000100c0   0x00000000   Code   RO         2667  * .ARM.Collect$$$$00000000  mc_p.l(entry.o)
    0x000100c0   0x000100c0   0x00000004   Code   RO         2973    .ARM.Collect$$$$00000001  mc_p.l(entry2.o)
    0x000100c4   0x000100c4   0x00000004   Code   RO         2976    .ARM.Collect$$$$00000004  mc_p.l(entry5.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         2978    .ARM.Collect$$$$00000008  mc_p.l(entry7b.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         2980    .ARM.Collect$$$$0000000A  mc_p.l(entry8b.o)
    0x000100c8   0x000100c8   0x00000008   Code   RO         2981    .ARM.Collect$$$$0000000B  mc_p.l(entry9a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         2983    .ARM.Collect$$$$0000000D  mc_p.l(entry10a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         2985    .ARM.Collect$$$$0000000F  mc_p.l(entry11a.o)
    0x000100d0   0x000100d0   0x00000004   Code   RO         2974    .ARM.Collect$$$$00002712  mc_p.l(entry2.o)
    0x000100d4   0x000100d4   0x00000078   Code   RO          539    .text               startup_armcm0.o
    0x0001014c   0x0001014c   0x0000002c   Code   RO         2670    .text               mc_p.l(uidiv.o)
    0x00010178   0x00010178   0x00000028   Code   RO         2672    .text               mc_p.l(idiv.o)
    0x000101a0   0x000101a0   0x00000024   Code   RO         2674    .text               mc_p.l(memcpya.o)
    0x000101c4   0x000101c4   0x00000024   Code   RO         2676    .text               mc_p.l(memseta.o)
    0x000101e8   0x000101e8   0x0000000e   Code   RO         2678    .text               mc_p.l(strlen.o)
    0x000101f6   0x000101f6   0x000000b2   Code   RO         2943    .text               mf_p.l(fadd.o)
    0x000102a8   0x000102a8   0x0000007a   Code   RO         2945    .text               mf_p.l(fmul.o)
    0x00010322   0x00010322   0x0000007c   Code   RO         2947    .text               mf_p.l(fdiv.o)
    0x0001039e   0x0001039e   0x00000018   Code   RO         2949    .text               mf_p.l(fscalb.o)
    0x000103b6   0x000103b6   0x00000002   PAD
    0x000103b8   0x000103b8   0x00000164   Code   RO         2951    .text               mf_p.l(dadd.o)
    0x0001051c   0x0001051c   0x000000d0   Code   RO         2953    .text               mf_p.l(dmul.o)
    0x000105ec   0x000105ec   0x000000f0   Code   RO         2955    .text               mf_p.l(ddiv.o)
    0x000106dc   0x000106dc   0x0000000e   Code   RO         2957    .text               mf_p.l(ffltui.o)
    0x000106ea   0x000106ea   0x00000002   PAD
    0x000106ec   0x000106ec   0x0000001c   Code   RO         2959    .text               mf_p.l(dfltui.o)
    0x00010708   0x00010708   0x00000028   Code   RO         2961    .text               mf_p.l(ffixui.o)
    0x00010730   0x00010730   0x0000003c   Code   RO         2963    .text               mf_p.l(dfixui.o)
    0x0001076c   0x0001076c   0x00000028   Code   RO         2965    .text               mf_p.l(f2d.o)
    0x00010794   0x00010794   0x00000038   Code   RO         2967    .text               mf_p.l(d2f.o)
    0x000107cc   0x000107cc   0x00000014   Code   RO         2969    .text               mf_p.l(cfcmple.o)
    0x000107e0   0x000107e0   0x00000014   Code   RO         2971    .text               mf_p.l(cfrcmple.o)
    0x000107f4   0x000107f4   0x00000060   Code   RO         2988    .text               mc_p.l(uldiv.o)
    0x00010854   0x00010854   0x00000020   Code   RO         2990    .text               mc_p.l(llshl.o)
    0x00010874   0x00010874   0x00000022   Code   RO         2992    .text               mc_p.l(llushr.o)
    0x00010896   0x00010896   0x00000026   Code   RO         2994    .text               mc_p.l(llsshr.o)
    0x000108bc   0x000108bc   0x00000000   Code   RO         2996    .text               mc_p.l(iusefp.o)
    0x000108bc   0x000108bc   0x00000082   Code   RO         2997    .text               mf_p.l(fepilogue.o)
    0x0001093e   0x0001093e   0x000000be   Code   RO         2999    .text               mf_p.l(depilogue.o)
    0x000109fc   0x000109fc   0x00000040   Code   RO         3003    .text               mf_p.l(dfixul.o)
    0x00010a3c   0x00010a3c   0x00000028   Code   RO         3005    .text               mf_p.l(cdrcmple.o)
    0x00010a64   0x00010a64   0x00000024   Code   RO         3007    .text               mc_p.l(init.o)
    0x00010a88   0x00010a88   0x00000056   Code   RO         3017    .text               mc_p.l(__dczerorl2.o)
    0x00010ade   0x00010ade   0x00000002   PAD
    0x00010ae0   0x00010ae0   0x0000001c   Code   RO         1641    i.AP_NRESET_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010afc   0x00010afc   0x0000005c   Code   RO         1568    i.DMA_IRQn_Handler  CVWL668.lib(drv_dma.o)
    0x00010b58   0x00010b58   0x0000000a   Code   RO         1642    i.EXTI_INT0_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010b62   0x00010b62   0x0000000a   Code   RO         1643    i.EXTI_INT1_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010b6c   0x00010b6c   0x0000000a   Code   RO         1644    i.EXTI_INT2_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010b76   0x00010b76   0x0000000a   Code   RO         1645    i.EXTI_INT3_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010b80   0x00010b80   0x0000000a   Code   RO         1646    i.EXTI_INT4_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010b8a   0x00010b8a   0x0000000a   Code   RO         1647    i.EXTI_INT5_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010b94   0x00010b94   0x0000000a   Code   RO         1648    i.EXTI_INT6_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010b9e   0x00010b9e   0x0000000a   Code   RO         1649    i.EXTI_INT7_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010ba8   0x00010ba8   0x00000048   Code   RO         1503    i.HardFault_Handler  CVWL668.lib(drv_common.o)
    0x00010bf0   0x00010bf0   0x0000000c   Code   RO         1995    i.I2C0_IRQn_Handler  CVWL668.lib(drv_i2c.o)
    0x00010bfc   0x00010bfc   0x0000000c   Code   RO         1996    i.I2C1_IRQn_Handler  CVWL668.lib(drv_i2c.o)
    0x00010c08   0x00010c08   0x0000000c   Code   RO         1997    i.I2C2_IRQn_Handler  CVWL668.lib(drv_i2c.o)
    0x00010c14   0x00010c14   0x000000e8   Code   RO         1352    i.LCDC_IRQn_Handler  CVWL668.lib(hal_internal_vsync.o)
    0x00010cfc   0x00010cfc   0x0000009a   Code   RO         2351    i.MEMC_IRQn_Handler  CVWL668.lib(drv_memc.o)
    0x00010d96   0x00010d96   0x00000002   PAD
    0x00010d98   0x00010d98   0x000000b8   Code   RO         2157    i.MIPI_TX_IRQn_Handler  CVWL668.lib(drv_dsi_tx.o)
    0x00010e50   0x00010e50   0x00000040   Code   RO         1135    i.SPIM_IRQn_Handler  CVWL668.lib(hal_spi_master.o)
    0x00010e90   0x00010e90   0x00000030   Code   RO         1836    i.SWIRE_IRQn_Handler  CVWL668.lib(drv_swire.o)
    0x00010ec0   0x00010ec0   0x00000018   Code   RO         1504    i.SysTick_Handler   CVWL668.lib(drv_common.o)
    0x00010ed8   0x00010ed8   0x0000000a   Code   RO         1897    i.TIMER0_IRQn_Handler  CVWL668.lib(drv_timer.o)
    0x00010ee2   0x00010ee2   0x0000000a   Code   RO         1898    i.TIMER1_IRQn_Handler  CVWL668.lib(drv_timer.o)
    0x00010eec   0x00010eec   0x0000000a   Code   RO         1899    i.TIMER2_IRQn_Handler  CVWL668.lib(drv_timer.o)
    0x00010ef6   0x00010ef6   0x0000000a   Code   RO         1900    i.TIMER3_IRQn_Handler  CVWL668.lib(drv_timer.o)
    0x00010f00   0x00010f00   0x0000001c   Code   RO         2504    i.VIDC_IRQn_Handler  CVWL668.lib(drv_vidc.o)
    0x00010f1c   0x00010f1c   0x0000001c   Code   RO         2417    i.VPRE1_IRQn_Handler  CVWL668.lib(drv_rxbr.o)
    0x00010f38   0x00010f38   0x0000006c   Code   RO         1414    i.VPRE_IRQn_Handler  CVWL668.lib(hal_internal_dcs.o)
    0x00010fa4   0x00010fa4   0x00000038   Code   RO         1930    i.WDG_IRQn_Handler  CVWL668.lib(drv_wdg.o)
    0x00010fdc   0x00010fdc   0x00000020   Code   RO         2915    i.__0printf         mc_p.l(printfa.o)
    0x00010ffc   0x00010ffc   0x00000002   Code   RO         3012    i.__scatterload_null  mc_p.l(handlers.o)
    0x00010ffe   0x00010ffe   0x00000002   PAD
    0x00011000   0x00011000   0x0000001c   Data   RO         1511    .ARM.__at_0x11000   CVWL668.lib(drv_common.o)
    0x0001101c   0x0001101c   0x00000010   Data   RO         1308    .ARM.__at_0x1101C   CVWL668.lib(tau_log.o)
    0x0001102c   0x0001102c   0x00000016   Data   RO         1011    .ARM.__at_0x1102C   CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00011042   0x00011042   0x00000002   PAD
    0x00011044   0x00011044   0x00000364   Code   RO         2096    i.MIPI_RX_IRQn_Handler  CVWL668.lib(drv_dsi_rx.o)
    0x000113a8   0x000113a8   0x00000180   Code   RO         2589    i.UART_IRQn_Handler  CVWL668.lib(drv_uart.o)
    0x00011528   0x00011528   0x00000024   Code   RO         2921    i.__0vsprintf       mc_p.l(printfa.o)
    0x0001154c   0x0001154c   0x0000002e   Code   RO         3001    i.__ARM_clz         mf_p.l(depilogue.o)
    0x0001157a   0x0001157a   0x0000001a   Code   RO          963    i.__ARM_common_switch8  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00011594   0x00011594   0x00000020   Code   RO         2418    i.__NVIC_DisableIRQ  CVWL668.lib(drv_rxbr.o)
    0x000115b4   0x000115b4   0x00000018   Code   RO         2419    i.__NVIC_EnableIRQ  CVWL668.lib(drv_rxbr.o)
    0x000115cc   0x000115cc   0x0000000e   Code   RO         3011    i.__scatterload_copy  mc_p.l(handlers.o)
    0x000115da   0x000115da   0x0000000e   Code   RO         3013    i.__scatterload_zeroinit  mc_p.l(handlers.o)
    0x000115e8   0x000115e8   0x00000174   Code   RO         2922    i._fp_digits        mc_p.l(printfa.o)
    0x0001175c   0x0001175c   0x000006ec   Code   RO         2923    i._printf_core      mc_p.l(printfa.o)
    0x00011e48   0x00011e48   0x00000020   Code   RO         2924    i._printf_post_padding  mc_p.l(printfa.o)
    0x00011e68   0x00011e68   0x0000002c   Code   RO         2925    i._printf_pre_padding  mc_p.l(printfa.o)
    0x00011e94   0x00011e94   0x0000000a   Code   RO         2927    i._sputc            mc_p.l(printfa.o)
    0x00011e9e   0x00011e9e   0x00000002   PAD
    0x00011ea0   0x00011ea0   0x000000b0   Code   RO          322    i.ap_dcs_set_backlight  s8_demo.o
    0x00011f50   0x00011f50   0x0000004c   Code   RO          323    i.ap_dcs_set_display_off  s8_demo.o
    0x00011f9c   0x00011f9c   0x0000003c   Code   RO          324    i.ap_dcs_set_display_on  s8_demo.o
    0x00011fd8   0x00011fd8   0x00000088   Code   RO          325    i.ap_dcs_set_enter_sleep_mode  s8_demo.o
    0x00012060   0x00012060   0x00000064   Code   RO          326    i.ap_dcs_set_exit_sleep_mode  s8_demo.o
    0x000120c4   0x000120c4   0x0000001c   Code   RO          329    i.ap_rstn_pull_high_cb  s8_demo.o
    0x000120e0   0x000120e0   0x00000054   Code   RO          330    i.ap_set_framerate  s8_demo.o
    0x00012134   0x00012134   0x00000084   Code   RO          331    i.ap_update_pps_9E  s8_demo.o
    0x000121b8   0x000121b8   0x00000068   Code   RO          332    i.app_display_init  s8_demo.o
    0x00012220   0x00012220   0x00000020   Code   RO          333    i.app_gpio_init     s8_demo.o
    0x00012240   0x00012240   0x00000048   Code   RO          334    i.app_init_panel    s8_demo.o
    0x00012288   0x00012288   0x000000e8   Code   RO          335    i.app_mipi_rx_init  s8_demo.o
    0x00012370   0x00012370   0x000000c0   Code   RO          337    i.app_mipi_tx_init  s8_demo.o
    0x00012430   0x00012430   0x0000006c   Code   RO          338    i.app_mipi_tx_start  s8_demo.o
    0x0001249c   0x0001249c   0x0000008c   Code   RO          339    i.app_set_dcs_hw_ack  s8_demo.o
    0x00012528   0x00012528   0x0000004c   Code   RO          340    i.app_system_process  s8_demo.o
    0x00012574   0x00012574   0x00000048   Code   RO          341    i.app_system_resume  s8_demo.o
    0x000125bc   0x000125bc   0x000000f4   Code   RO          342    i.app_system_suspend  s8_demo.o
    0x000126b0   0x000126b0   0x0000002e   Code   RO          343    i.app_tx_panel_reset  s8_demo.o
    0x000126de   0x000126de   0x00000002   PAD
    0x000126e0   0x000126e0   0x0000002c   Code   RO          518    i.board_Init        board.o
    0x0001270c   0x0001270c   0x000000c8   Code   RO         2664    i.ceil              m_ps.l(ceil.o)
    0x000127d4   0x000127d4   0x0000002c   Code   RO         1353    i.check_mipi_rx_tx_video_info  CVWL668.lib(hal_internal_vsync.o)
    0x00012800   0x00012800   0x00000088   Code   RO         1415    i.check_pkt_buf_rev  CVWL668.lib(hal_internal_dcs.o)
    0x00012888   0x00012888   0x00000058   Code   RO         2062    i.dcs_packet_fifo_alloc  CVWL668.lib(dcs_packet_fifo.o)
    0x000128e0   0x000128e0   0x00000018   Code   RO         2063    i.dcs_packet_fifo_init  CVWL668.lib(dcs_packet_fifo.o)
    0x000128f8   0x000128f8   0x00000044   Code   RO         2064    i.dcs_packet_free_fifo_header  CVWL668.lib(dcs_packet_fifo.o)
    0x0001293c   0x0001293c   0x00000024   Code   RO         2065    i.dcs_packet_get_fifo_header  CVWL668.lib(dcs_packet_fifo.o)
    0x00012960   0x00012960   0x00000018   Code   RO         1295    i.delayMs           CVWL668.lib(tau_delay.o)
    0x00012978   0x00012978   0x0000002c   Code   RO         1296    i.delayUs           CVWL668.lib(tau_delay.o)
    0x000129a4   0x000129a4   0x00000008   Code   RO         1509    i.drv_common_system_init  CVWL668.lib(drv_common.o)
    0x000129ac   0x000129ac   0x0000003c   Code   RO         1528    i.drv_crgu_enable_clock  CVWL668.lib(drv_crgu.o)
    0x000129e8   0x000129e8   0x00000068   Code   RO         1531    i.drv_crgu_get_rxbr_clk  CVWL668.lib(drv_crgu.o)
    0x00012a50   0x00012a50   0x00000010   Code   RO         1534    i.drv_crgu_reset_modules  CVWL668.lib(drv_crgu.o)
    0x00012a60   0x00012a60   0x00000028   Code   RO         1535    i.drv_crgu_set_ahb_clk  CVWL668.lib(drv_crgu.o)
    0x00012a88   0x00012a88   0x00000010   Code   RO         1536    i.drv_crgu_set_clock_div  CVWL668.lib(drv_crgu.o)
    0x00012a98   0x00012a98   0x0000003c   Code   RO         1538    i.drv_crgu_set_dpi_clk  CVWL668.lib(drv_crgu.o)
    0x00012ad4   0x00012ad4   0x00000038   Code   RO         1539    i.drv_crgu_set_dsc_clk  CVWL668.lib(drv_crgu.o)
    0x00012b0c   0x00012b0c   0x00000028   Code   RO         1540    i.drv_crgu_set_fb_clk  CVWL668.lib(drv_crgu.o)
    0x00012b34   0x00012b34   0x00000028   Code   RO         1541    i.drv_crgu_set_lcdc_clk  CVWL668.lib(drv_crgu.o)
    0x00012b5c   0x00012b5c   0x00000018   Code   RO         1542    i.drv_crgu_set_reset  CVWL668.lib(drv_crgu.o)
    0x00012b74   0x00012b74   0x00000028   Code   RO         1543    i.drv_crgu_set_rxbr_clk  CVWL668.lib(drv_crgu.o)
    0x00012b9c   0x00012b9c   0x00000028   Code   RO         1544    i.drv_crgu_set_vidc_clk  CVWL668.lib(drv_crgu.o)
    0x00012bc4   0x00012bc4   0x00000018   Code   RO         1570    i.drv_dma_clear_status  CVWL668.lib(drv_dma.o)
    0x00012bdc   0x00012bdc   0x00000014   Code   RO         1576    i.drv_dma_get_int_source  CVWL668.lib(drv_dma.o)
    0x00012bf0   0x00012bf0   0x0000001c   Code   RO         1631    i.drv_dsc_dec_disable  CVWL668.lib(drv_dsc_dec.o)
    0x00012c0c   0x00012c0c   0x0000003c   Code   RO         1632    i.drv_dsc_dec_enable  CVWL668.lib(drv_dsc_dec.o)
    0x00012c48   0x00012c48   0x00000020   Code   RO         1633    i.drv_dsc_dec_get_nslc  CVWL668.lib(drv_dsc_dec.o)
    0x00012c68   0x00012c68   0x0000010c   Code   RO         2097    i.drv_dsi_rx_calc_ipi_tx_delay  CVWL668.lib(drv_dsi_rx.o)
    0x00012d74   0x00012d74   0x00000040   Code   RO         2098    i.drv_dsi_rx_enable_irq  CVWL668.lib(drv_dsi_rx.o)
    0x00012db4   0x00012db4   0x00000050   Code   RO         2100    i.drv_dsi_rx_get_color_bpp  CVWL668.lib(drv_dsi_rx.o)
    0x00012e04   0x00012e04   0x0000001c   Code   RO         2101    i.drv_dsi_rx_get_color_pcc  CVWL668.lib(drv_dsi_rx.o)
    0x00012e20   0x00012e20   0x00000010   Code   RO         2102    i.drv_dsi_rx_get_compression_en  CVWL668.lib(drv_dsi_rx.o)
    0x00012e30   0x00012e30   0x00000010   Code   RO         2103    i.drv_dsi_rx_get_ddi_crc_en  CVWL668.lib(drv_dsi_rx.o)
    0x00012e40   0x00012e40   0x00000018   Code   RO         2108    i.drv_dsi_rx_power_up  CVWL668.lib(drv_dsi_rx.o)
    0x00012e58   0x00012e58   0x0000001c   Code   RO         2109    i.drv_dsi_rx_set_check_crc  CVWL668.lib(drv_dsi_rx.o)
    0x00012e74   0x00012e74   0x00000024   Code   RO         2110    i.drv_dsi_rx_set_ctrl_cfg  CVWL668.lib(drv_dsi_rx.o)
    0x00012e98   0x00012e98   0x00000010   Code   RO         2111    i.drv_dsi_rx_set_ddi_cfg  CVWL668.lib(drv_dsi_rx.o)
    0x00012ea8   0x00012ea8   0x0000001c   Code   RO         2112    i.drv_dsi_rx_set_ddi_crc_en  CVWL668.lib(drv_dsi_rx.o)
    0x00012ec4   0x00012ec4   0x0000000c   Code   RO         2115    i.drv_dsi_rx_set_inten  CVWL668.lib(drv_dsi_rx.o)
    0x00012ed0   0x00012ed0   0x00000010   Code   RO         2116    i.drv_dsi_rx_set_ipi_cfg  CVWL668.lib(drv_dsi_rx.o)
    0x00012ee0   0x00012ee0   0x0000001c   Code   RO         2118    i.drv_dsi_rx_set_ipi_ycbcr_frmt  CVWL668.lib(drv_dsi_rx.o)
    0x00012efc   0x00012efc   0x00000014   Code   RO         2119    i.drv_dsi_rx_set_lane_swap  CVWL668.lib(drv_dsi_rx.o)
    0x00012f10   0x00012f10   0x00000024   Code   RO         2120    i.drv_dsi_rx_set_resp_cnt  CVWL668.lib(drv_dsi_rx.o)
    0x00012f34   0x00012f34   0x0000001c   Code   RO         2121    i.drv_dsi_rx_set_tear_resp_en  CVWL668.lib(drv_dsi_rx.o)
    0x00012f50   0x00012f50   0x00000098   Code   RO         2122    i.drv_dsi_rx_set_up_phy  CVWL668.lib(drv_dsi_rx.o)
    0x00012fe8   0x00012fe8   0x00000018   Code   RO         2123    i.drv_dsi_rx_shut_down  CVWL668.lib(drv_dsi_rx.o)
    0x00013000   0x00013000   0x00000018   Code   RO         2159    i.drv_dsi_tx_command_header  CVWL668.lib(drv_dsi_tx.o)
    0x00013018   0x00013018   0x00000058   Code   RO         2160    i.drv_dsi_tx_command_mode_cfg  CVWL668.lib(drv_dsi_tx.o)
    0x00013070   0x00013070   0x0000000c   Code   RO         2161    i.drv_dsi_tx_command_put_payload  CVWL668.lib(drv_dsi_tx.o)
    0x0001307c   0x0001307c   0x00000020   Code   RO         2162    i.drv_dsi_tx_config_eotp  CVWL668.lib(drv_dsi_tx.o)
    0x0001309c   0x0001309c   0x0000000c   Code   RO         2163    i.drv_dsi_tx_config_int  CVWL668.lib(drv_dsi_tx.o)
    0x000130a8   0x000130a8   0x00000010   Code   RO         2164    i.drv_dsi_tx_dpi_lpcmd_time  CVWL668.lib(drv_dsi_tx.o)
    0x000130b8   0x000130b8   0x00000010   Code   RO         2165    i.drv_dsi_tx_dpi_mode  CVWL668.lib(drv_dsi_tx.o)
    0x000130c8   0x000130c8   0x00000024   Code   RO         2166    i.drv_dsi_tx_dpi_polarity  CVWL668.lib(drv_dsi_tx.o)
    0x000130ec   0x000130ec   0x0000000c   Code   RO         2167    i.drv_dsi_tx_edpi_cmd_size  CVWL668.lib(drv_dsi_tx.o)
    0x000130f8   0x000130f8   0x0000000c   Code   RO         2169    i.drv_dsi_tx_get_cmd_status  CVWL668.lib(drv_dsi_tx.o)
    0x00013104   0x00013104   0x0000000c   Code   RO         2171    i.drv_dsi_tx_mode   CVWL668.lib(drv_dsi_tx.o)
    0x00013110   0x00013110   0x0000001c   Code   RO         2172    i.drv_dsi_tx_phy_clock_lane_auto_lp  CVWL668.lib(drv_dsi_tx.o)
    0x0001312c   0x0001312c   0x00000020   Code   RO         2173    i.drv_dsi_tx_phy_clock_lane_req_hs  CVWL668.lib(drv_dsi_tx.o)
    0x0001314c   0x0001314c   0x00000010   Code   RO         2175    i.drv_dsi_tx_phy_lane_mode  CVWL668.lib(drv_dsi_tx.o)
    0x0001315c   0x0001315c   0x00000068   Code   RO         2178    i.drv_dsi_tx_phy_status_ready  CVWL668.lib(drv_dsi_tx.o)
    0x000131c4   0x000131c4   0x00000044   Code   RO         2179    i.drv_dsi_tx_phy_status_stopstate  CVWL668.lib(drv_dsi_tx.o)
    0x00013208   0x00013208   0x00000150   Code   RO         2181    i.drv_dsi_tx_phy_test_setup  CVWL668.lib(drv_dsi_tx.o)
    0x00013358   0x00013358   0x00000020   Code   RO         2182    i.drv_dsi_tx_phy_time_cfg  CVWL668.lib(drv_dsi_tx.o)
    0x00013378   0x00013378   0x0000000c   Code   RO         2186    i.drv_dsi_tx_powerup  CVWL668.lib(drv_dsi_tx.o)
    0x00013384   0x00013384   0x00000024   Code   RO         2187    i.drv_dsi_tx_response_mode  CVWL668.lib(drv_dsi_tx.o)
    0x000133a8   0x000133a8   0x0000001c   Code   RO         2190    i.drv_dsi_tx_set_bta_ack  CVWL668.lib(drv_dsi_tx.o)
    0x000133c4   0x000133c4   0x00000014   Code   RO         2191    i.drv_dsi_tx_set_esc_div  CVWL668.lib(drv_dsi_tx.o)
    0x000133d8   0x000133d8   0x00000040   Code   RO         2192    i.drv_dsi_tx_set_int  CVWL668.lib(drv_dsi_tx.o)
    0x00013418   0x00013418   0x00000018   Code   RO         2193    i.drv_dsi_tx_set_time_out_div  CVWL668.lib(drv_dsi_tx.o)
    0x00013430   0x00013430   0x00000014   Code   RO         2194    i.drv_dsi_tx_set_video_chunk  CVWL668.lib(drv_dsi_tx.o)
    0x00013444   0x00013444   0x00000024   Code   RO         2195    i.drv_dsi_tx_set_video_timing  CVWL668.lib(drv_dsi_tx.o)
    0x00013468   0x00013468   0x0000000c   Code   RO         2197    i.drv_dsi_tx_shutdown  CVWL668.lib(drv_dsi_tx.o)
    0x00013474   0x00013474   0x0000002c   Code   RO         2198    i.drv_dsi_tx_timeout_cfg  CVWL668.lib(drv_dsi_tx.o)
    0x000134a0   0x000134a0   0x000000e8   Code   RO         2201    i.drv_dsi_tx_video_mode_cfg  CVWL668.lib(drv_dsi_tx.o)
    0x00013588   0x00013588   0x00000036   Code   RO         2634    i.drv_efuse_enter_inactive  CVWL668.lib(drv_efuse.o)
    0x000135be   0x000135be   0x0000000c   Code   RO         2637    i.drv_efuse_int_enable  CVWL668.lib(drv_efuse.o)
    0x000135ca   0x000135ca   0x0000003a   Code   RO         2638    i.drv_efuse_read    CVWL668.lib(drv_efuse.o)
    0x00013604   0x00013604   0x00000018   Code   RO         2639    i.drv_efuse_read_req  CVWL668.lib(drv_efuse.o)
    0x0001361c   0x0001361c   0x00000010   Code   RO         1650    i.drv_gpio_get_attribute  CVWL668.lib(drv_gpio.o)
    0x0001362c   0x0001362c   0x00000024   Code   RO         1652    i.drv_gpio_handle_int  CVWL668.lib(drv_gpio.o)
    0x00013650   0x00013650   0x0000000c   Code   RO         1653    i.drv_gpio_register_ap_reset_callback  CVWL668.lib(drv_gpio.o)
    0x0001365c   0x0001365c   0x00000014   Code   RO         1654    i.drv_gpio_register_callback  CVWL668.lib(drv_gpio.o)
    0x00013670   0x00013670   0x0000001c   Code   RO         1655    i.drv_gpio_set_attribute  CVWL668.lib(drv_gpio.o)
    0x0001368c   0x0001368c   0x00000044   Code   RO         1656    i.drv_gpio_set_int  CVWL668.lib(drv_gpio.o)
    0x000136d0   0x000136d0   0x00000020   Code   RO         1657    i.drv_gpio_set_ioe  CVWL668.lib(drv_gpio.o)
    0x000136f0   0x000136f0   0x00000014   Code   RO         1658    i.drv_gpio_set_mode  CVWL668.lib(drv_gpio.o)
    0x00013704   0x00013704   0x00000020   Code   RO         1063    i.drv_gpio_set_output_data  CVWL668.lib(hal_gpio.o)
    0x00013724   0x00013724   0x00000028   Code   RO         2263    i.drv_lcdc_bcsa_config  CVWL668.lib(drv_lcdc.o)
    0x0001374c   0x0001374c   0x0000002c   Code   RO         2264    i.drv_lcdc_cfg_int_frame  CVWL668.lib(drv_lcdc.o)
    0x00013778   0x00013778   0x00000018   Code   RO         2265    i.drv_lcdc_clear_int  CVWL668.lib(drv_lcdc.o)
    0x00013790   0x00013790   0x00000034   Code   RO         2267    i.drv_lcdc_cmd_start  CVWL668.lib(drv_lcdc.o)
    0x000137c4   0x000137c4   0x00000014   Code   RO         2268    i.drv_lcdc_config_acc_command_mode  CVWL668.lib(drv_lcdc.o)
    0x000137d8   0x000137d8   0x00000038   Code   RO         2269    i.drv_lcdc_config_int  CVWL668.lib(drv_lcdc.o)
    0x00013810   0x00013810   0x00000028   Code   RO         2270    i.drv_lcdc_config_int_single  CVWL668.lib(drv_lcdc.o)
    0x00013838   0x00013838   0x00000018   Code   RO         2271    i.drv_lcdc_config_overwrite_rgb  CVWL668.lib(drv_lcdc.o)
    0x00013850   0x00013850   0x00000050   Code   RO         2272    i.drv_lcdc_config_src_parameter  CVWL668.lib(drv_lcdc.o)
    0x000138a0   0x000138a0   0x00000010   Code   RO         2273    i.drv_lcdc_crop_hact  CVWL668.lib(drv_lcdc.o)
    0x000138b0   0x000138b0   0x00000038   Code   RO         2274    i.drv_lcdc_ctrl_flow  CVWL668.lib(drv_lcdc.o)
    0x000138e8   0x000138e8   0x00000030   Code   RO         2275    i.drv_lcdc_dith_config  CVWL668.lib(drv_lcdc.o)
    0x00013918   0x00013918   0x0000003c   Code   RO         2277    i.drv_lcdc_edge_dect_config  CVWL668.lib(drv_lcdc.o)
    0x00013954   0x00013954   0x00000064   Code   RO         2278    i.drv_lcdc_edge_enh_config  CVWL668.lib(drv_lcdc.o)
    0x000139b8   0x000139b8   0x00000024   Code   RO         2279    i.drv_lcdc_enable_shadow_reg  CVWL668.lib(drv_lcdc.o)
    0x000139dc   0x000139dc   0x0000001c   Code   RO         2280    i.drv_lcdc_endianness_config  CVWL668.lib(drv_lcdc.o)
    0x000139f8   0x000139f8   0x00000020   Code   RO         2281    i.drv_lcdc_fc_config  CVWL668.lib(drv_lcdc.o)
    0x00013a18   0x00013a18   0x00000024   Code   RO         2283    i.drv_lcdc_fldc_config  CVWL668.lib(drv_lcdc.o)
    0x00013a3c   0x00013a3c   0x00000024   Code   RO         2284    i.drv_lcdc_function_disable  CVWL668.lib(drv_lcdc.o)
    0x00013a60   0x00013a60   0x00000024   Code   RO         2285    i.drv_lcdc_function_enable  CVWL668.lib(drv_lcdc.o)
    0x00013a84   0x00013a84   0x0000003c   Code   RO         2296    i.drv_lcdc_set_int  CVWL668.lib(drv_lcdc.o)
    0x00013ac0   0x00013ac0   0x0000001c   Code   RO         2297    i.drv_lcdc_set_prefetch  CVWL668.lib(drv_lcdc.o)
    0x00013adc   0x00013adc   0x0000001c   Code   RO         2298    i.drv_lcdc_set_tear_line  CVWL668.lib(drv_lcdc.o)
    0x00013af8   0x00013af8   0x00000010   Code   RO         2300    i.drv_lcdc_stop_display  CVWL668.lib(drv_lcdc.o)
    0x00013b08   0x00013b08   0x0000003c   Code   RO         2302    i.drv_lcdc_vid_hw_start  CVWL668.lib(drv_lcdc.o)
    0x00013b44   0x00013b44   0x00000018   Code   RO         2304    i.drv_lcdc_vintp_mode_config  CVWL668.lib(drv_lcdc.o)
    0x00013b5c   0x00013b5c   0x00000014   Code   RO         2352    i.drv_memc_clear_status  CVWL668.lib(drv_memc.o)
    0x00013b70   0x00013b70   0x00000040   Code   RO         2353    i.drv_memc_enable_irq  CVWL668.lib(drv_memc.o)
    0x00013bb0   0x00013bb0   0x00000010   Code   RO         2354    i.drv_memc_gen_a_tear_signal  CVWL668.lib(drv_memc.o)
    0x00013bc0   0x00013bc0   0x00000018   Code   RO         2355    i.drv_memc_get_status  CVWL668.lib(drv_memc.o)
    0x00013bd8   0x00013bd8   0x00000010   Code   RO         2356    i.drv_memc_get_tear_mode  CVWL668.lib(drv_memc.o)
    0x00013be8   0x00013be8   0x0000001c   Code   RO         2357    i.drv_memc_rate_transfer_sel  CVWL668.lib(drv_memc.o)
    0x00013c04   0x00013c04   0x00000014   Code   RO         2358    i.drv_memc_sel_vsync  CVWL668.lib(drv_memc.o)
    0x00013c18   0x00013c18   0x00000018   Code   RO         2359    i.drv_memc_set_active_height  CVWL668.lib(drv_memc.o)
    0x00013c30   0x00013c30   0x0000001c   Code   RO         2360    i.drv_memc_set_circ_mode_enable  CVWL668.lib(drv_memc.o)
    0x00013c4c   0x00013c4c   0x00000014   Code   RO         2361    i.drv_memc_set_data_mode  CVWL668.lib(drv_memc.o)
    0x00013c60   0x00013c60   0x00000018   Code   RO         2364    i.drv_memc_set_double_buffer  CVWL668.lib(drv_memc.o)
    0x00013c78   0x00013c78   0x0000001c   Code   RO         2368    i.drv_memc_set_frame_drop_select  CVWL668.lib(drv_memc.o)
    0x00013c94   0x00013c94   0x00000018   Code   RO         2369    i.drv_memc_set_fs_en_conditions  CVWL668.lib(drv_memc.o)
    0x00013cac   0x00013cac   0x0000001c   Code   RO         2371    i.drv_memc_set_lcdc_st_conditions  CVWL668.lib(drv_memc.o)
    0x00013cc8   0x00013cc8   0x00000020   Code   RO         2372    i.drv_memc_set_ltpo_mode  CVWL668.lib(drv_memc.o)
    0x00013ce8   0x00013ce8   0x00000018   Code   RO         2373    i.drv_memc_set_ltpo_pu_thres  CVWL668.lib(drv_memc.o)
    0x00013d00   0x00013d00   0x00000014   Code   RO         2377    i.drv_memc_set_tear_mode  CVWL668.lib(drv_memc.o)
    0x00013d14   0x00013d14   0x0000002c   Code   RO         2378    i.drv_memc_set_tear_waveform  CVWL668.lib(drv_memc.o)
    0x00013d40   0x00013d40   0x00000014   Code   RO         2380    i.drv_memc_set_vidc_sync_cnt  CVWL668.lib(drv_memc.o)
    0x00013d54   0x00013d54   0x00000010   Code   RO         2657    i.drv_phy_test_clear  CVWL668.lib(drv_phy_common.o)
    0x00013d64   0x00013d64   0x00000018   Code   RO         2658    i.drv_phy_test_lock  CVWL668.lib(drv_phy_common.o)
    0x00013d7c   0x00013d7c   0x00000030   Code   RO         1688    i.drv_pwr_efuse_pd  CVWL668.lib(drv_pwr.o)
    0x00013dac   0x00013dac   0x00000040   Code   RO         1690    i.drv_pwr_enter_deep_sleep_mode  CVWL668.lib(drv_pwr.o)
    0x00013dec   0x00013dec   0x00000028   Code   RO         1692    i.drv_pwr_enter_sleep_mode_ex  CVWL668.lib(drv_pwr.o)
    0x00013e14   0x00013e14   0x0000008c   Code   RO         1693    i.drv_pwr_enter_stop_sleep_mode  CVWL668.lib(drv_pwr.o)
    0x00013ea0   0x00013ea0   0x00000028   Code   RO         1694    i.drv_pwr_exit_sleep_mode  CVWL668.lib(drv_pwr.o)
    0x00013ec8   0x00013ec8   0x00000010   Code   RO         1697    i.drv_pwr_get_power_ready_st  CVWL668.lib(drv_pwr.o)
    0x00013ed8   0x00013ed8   0x00000028   Code   RO         1729    i.drv_pwr_set_breath_screen_power_sel  CVWL668.lib(drv_pwr.o)
    0x00013f00   0x00013f00   0x00000028   Code   RO         1730    i.drv_pwr_set_digit_power_sel  CVWL668.lib(drv_pwr.o)
    0x00013f28   0x00013f28   0x00000034   Code   RO         1733    i.drv_pwr_set_pll_clk  CVWL668.lib(drv_pwr.o)
    0x00013f5c   0x00013f5c   0x0000002c   Code   RO         1736    i.drv_pwr_set_wakeup_type  CVWL668.lib(drv_pwr.o)
    0x00013f88   0x00013f88   0x00000020   Code   RO         1739    i.drv_pwr_write_lock  CVWL668.lib(drv_pwr.o)
    0x00013fa8   0x00013fa8   0x00000010   Code   RO         2420    i.drv_rxbr_clear_pkt_buffer  CVWL668.lib(drv_rxbr.o)
    0x00013fb8   0x00013fb8   0x0000000c   Code   RO         2421    i.drv_rxbr_clear_status0  CVWL668.lib(drv_rxbr.o)
    0x00013fc4   0x00013fc4   0x0000005a   Code   RO         2424    i.drv_rxbr_enable_irq  CVWL668.lib(drv_rxbr.o)
    0x0001401e   0x0001401e   0x00000002   PAD
    0x00014020   0x00014020   0x0000001c   Code   RO         2425    i.drv_rxbr_frame_drop_cfg  CVWL668.lib(drv_rxbr.o)
    0x0001403c   0x0001403c   0x00000018   Code   RO         1354    i.drv_rxbr_get_int_source  CVWL668.lib(hal_internal_vsync.o)
    0x00014054   0x00014054   0x00000018   Code   RO         1416    i.drv_rxbr_get_status0  CVWL668.lib(hal_internal_dcs.o)
    0x0001406c   0x0001406c   0x00000014   Code   RO         2435    i.drv_rxbr_hline_rcv1_cfg  CVWL668.lib(drv_rxbr.o)
    0x00014080   0x00014080   0x00000010   Code   RO         2436    i.drv_rxbr_hline_rcv_cfg  CVWL668.lib(drv_rxbr.o)
    0x00014090   0x00014090   0x0000000c   Code   RO         2438    i.drv_rxbr_register_irq1_callback  CVWL668.lib(drv_rxbr.o)
    0x0001409c   0x0001409c   0x00000144   Code   RO         2442    i.drv_rxbr_set_cmd_response  CVWL668.lib(drv_rxbr.o)
    0x000141e0   0x000141e0   0x0000001c   Code   RO         2444    i.drv_rxbr_set_color_format  CVWL668.lib(drv_rxbr.o)
    0x000141fc   0x000141fc   0x00000024   Code   RO         2447    i.drv_rxbr_set_filter_regs  CVWL668.lib(drv_rxbr.o)
    0x00014220   0x00014220   0x0000001c   Code   RO         2448    i.drv_rxbr_set_inten  CVWL668.lib(drv_rxbr.o)
    0x0001423c   0x0001423c   0x00000018   Code   RO         2449    i.drv_rxbr_set_ltpo_drop_th  CVWL668.lib(drv_rxbr.o)
    0x00014254   0x00014254   0x00000040   Code   RO         2453    i.drv_rxbr_set_usr_cfg  CVWL668.lib(drv_rxbr.o)
    0x00014294   0x00014294   0x00000010   Code   RO         2454    i.drv_rxbr_set_usr_col  CVWL668.lib(drv_rxbr.o)
    0x000142a4   0x000142a4   0x00000010   Code   RO         2455    i.drv_rxbr_set_usr_row  CVWL668.lib(drv_rxbr.o)
    0x000142b4   0x000142b4   0x00000078   Code   RO         2077    i.drv_se_init       CVWL668.lib(drv_se.o)
    0x0001432c   0x0001432c   0x000000d4   Code   RO         2078    i.drv_se_set_dsc    CVWL668.lib(drv_se.o)
    0x00014400   0x00014400   0x00000088   Code   RO         2079    i.drv_se_set_lcdc   CVWL668.lib(drv_se.o)
    0x00014488   0x00014488   0x00000090   Code   RO         2080    i.drv_se_set_memc   CVWL668.lib(drv_se.o)
    0x00014518   0x00014518   0x000000d0   Code   RO         2081    i.drv_se_set_rxbr   CVWL668.lib(drv_se.o)
    0x000145e8   0x000145e8   0x000000ac   Code   RO         2082    i.drv_se_set_vidc   CVWL668.lib(drv_se.o)
    0x00014694   0x00014694   0x00000014   Code   RO         2083    i.drv_se_start_rx   CVWL668.lib(drv_se.o)
    0x000146a8   0x000146a8   0x0000000c   Code   RO         1801    i.drv_spim_clear_int_status  CVWL668.lib(drv_spi_master.o)
    0x000146b4   0x000146b4   0x00000030   Code   RO         1804    i.drv_spim_disable_int  CVWL668.lib(drv_spi_master.o)
    0x000146e4   0x000146e4   0x00000010   Code   RO         1809    i.drv_spim_get_busy  CVWL668.lib(drv_spi_master.o)
    0x000146f4   0x000146f4   0x0000000c   Code   RO         1810    i.drv_spim_get_int_status  CVWL668.lib(drv_spi_master.o)
    0x00014700   0x00014700   0x0000001c   Code   RO         1814    i.drv_spim_set_inten  CVWL668.lib(drv_spi_master.o)
    0x0001471c   0x0001471c   0x0000001c   Code   RO         1837    i.drv_swire_enable  CVWL668.lib(drv_swire.o)
    0x00014738   0x00014738   0x0000000c   Code   RO         1838    i.drv_swire_get_pulse_count  CVWL668.lib(drv_swire.o)
    0x00014744   0x00014744   0x0000000c   Code   RO         1839    i.drv_swire_register_callback  CVWL668.lib(drv_swire.o)
    0x00014750   0x00014750   0x00000018   Code   RO         1840    i.drv_swire_set_bit_time  CVWL668.lib(drv_swire.o)
    0x00014768   0x00014768   0x00000048   Code   RO         1841    i.drv_swire_set_int  CVWL668.lib(drv_swire.o)
    0x000147b0   0x000147b0   0x0000001c   Code   RO         1842    i.drv_swire_set_power_down  CVWL668.lib(drv_swire.o)
    0x000147cc   0x000147cc   0x0000000c   Code   RO         1843    i.drv_swire_set_pulse_count  CVWL668.lib(drv_swire.o)
    0x000147d8   0x000147d8   0x0000001c   Code   RO         1844    i.drv_swire_set_trig_mode  CVWL668.lib(drv_swire.o)
    0x000147f4   0x000147f4   0x0000000c   Code   RO         1860    i.drv_sys_cfg_clear_all_int  CVWL668.lib(drv_sys_cfg.o)
    0x00014800   0x00014800   0x00000028   Code   RO         1861    i.drv_sys_cfg_clear_pending  CVWL668.lib(drv_sys_cfg.o)
    0x00014828   0x00014828   0x00000024   Code   RO         1868    i.drv_sys_cfg_sel_ap_rst_trig  CVWL668.lib(drv_sys_cfg.o)
    0x0001484c   0x0001484c   0x00000024   Code   RO         1870    i.drv_sys_cfg_sel_gpio_group  CVWL668.lib(drv_sys_cfg.o)
    0x00014870   0x00014870   0x00000024   Code   RO         1871    i.drv_sys_cfg_sel_int_trig  CVWL668.lib(drv_sys_cfg.o)
    0x00014894   0x00014894   0x00000018   Code   RO         1872    i.drv_sys_cfg_sel_swire_timer  CVWL668.lib(drv_sys_cfg.o)
    0x000148ac   0x000148ac   0x00000024   Code   RO         1875    i.drv_sys_cfg_set_int  CVWL668.lib(drv_sys_cfg.o)
    0x000148d0   0x000148d0   0x0000001a   Code   RO         1901    i.drv_timer_clear_status_flags  CVWL668.lib(drv_timer.o)
    0x000148ea   0x000148ea   0x00000020   Code   RO         1902    i.drv_timer_enable  CVWL668.lib(drv_timer.o)
    0x0001490a   0x0001490a   0x00000002   PAD
    0x0001490c   0x0001490c   0x00000010   Code   RO         1903    i.drv_timer_get_instance  CVWL668.lib(drv_timer.o)
    0x0001491c   0x0001491c   0x0000003c   Code   RO         1905    i.drv_timer_handle_interrupt  CVWL668.lib(drv_timer.o)
    0x00014958   0x00014958   0x00000014   Code   RO         1906    i.drv_timer_register_callback  CVWL668.lib(drv_timer.o)
    0x0001496c   0x0001496c   0x00000040   Code   RO         1907    i.drv_timer_set_compare_val  CVWL668.lib(drv_timer.o)
    0x000149ac   0x000149ac   0x00000048   Code   RO         1908    i.drv_timer_set_int  CVWL668.lib(drv_timer.o)
    0x000149f4   0x000149f4   0x00000028   Code   RO         1909    i.drv_timer_set_prescaler  CVWL668.lib(drv_timer.o)
    0x00014a1c   0x00014a1c   0x00000010   Code   RO         1910    i.drv_timer_set_repeat  CVWL668.lib(drv_timer.o)
    0x00014a2c   0x00014a2c   0x00000020   Code   RO         2203    i.drv_tx_phy_test_enter  CVWL668.lib(drv_dsi_tx.o)
    0x00014a4c   0x00014a4c   0x00000020   Code   RO         2204    i.drv_tx_phy_test_exit  CVWL668.lib(drv_dsi_tx.o)
    0x00014a6c   0x00014a6c   0x00000028   Code   RO         2207    i.drv_tx_phy_test_write_code  CVWL668.lib(drv_dsi_tx.o)
    0x00014a94   0x00014a94   0x00000034   Code   RO         2590    i.drv_uart_abort_recv  CVWL668.lib(drv_uart.o)
    0x00014ac8   0x00014ac8   0x00000034   Code   RO         2591    i.drv_uart_abort_send  CVWL668.lib(drv_uart.o)
    0x00014afc   0x00014afc   0x00000014   Code   RO         2592    i.drv_uart_config_int  CVWL668.lib(drv_uart.o)
    0x00014b10   0x00014b10   0x00000018   Code   RO         2594    i.drv_uart_enable_clk  CVWL668.lib(drv_uart.o)
    0x00014b28   0x00014b28   0x0000005c   Code   RO         2595    i.drv_uart_enable_int  CVWL668.lib(drv_uart.o)
    0x00014b84   0x00014b84   0x00000028   Code   RO         2597    i.drv_uart_get_instance  CVWL668.lib(drv_uart.o)
    0x00014bac   0x00014bac   0x000000ce   Code   RO         2598    i.drv_uart_init     CVWL668.lib(drv_uart.o)
    0x00014c7a   0x00014c7a   0x00000002   PAD
    0x00014c7c   0x00014c7c   0x0000003c   Code   RO         2599    i.drv_uart_int_trans_handle  CVWL668.lib(drv_uart.o)
    0x00014cb8   0x00014cb8   0x0000001c   Code   RO         2602    i.drv_uart_reset_rx_fifo  CVWL668.lib(drv_uart.o)
    0x00014cd4   0x00014cd4   0x0000001c   Code   RO         2603    i.drv_uart_reset_tx_fifo  CVWL668.lib(drv_uart.o)
    0x00014cf0   0x00014cf0   0x0000001a   Code   RO         2604    i.drv_uart_send_blocking  CVWL668.lib(drv_uart.o)
    0x00014d0a   0x00014d0a   0x00000054   Code   RO         2606    i.drv_uart_set_baud_rate  CVWL668.lib(drv_uart.o)
    0x00014d5e   0x00014d5e   0x00000002   PAD
    0x00014d60   0x00014d60   0x0000004c   Code   RO         2607    i.drv_uart_trans_create_handle  CVWL668.lib(drv_uart.o)
    0x00014dac   0x00014dac   0x00000010   Code   RO         2505    i.drv_vidc_clear_irq  CVWL668.lib(drv_vidc.o)
    0x00014dbc   0x00014dbc   0x00000020   Code   RO         2509    i.drv_vidc_enable   CVWL668.lib(drv_vidc.o)
    0x00014ddc   0x00014ddc   0x00000040   Code   RO         2510    i.drv_vidc_enable_irq  CVWL668.lib(drv_vidc.o)
    0x00014e1c   0x00014e1c   0x0000002c   Code   RO         2511    i.drv_vidc_get_int_source  CVWL668.lib(drv_vidc.o)
    0x00014e48   0x00014e48   0x00000018   Code   RO         2512    i.drv_vidc_get_irq_status  CVWL668.lib(drv_vidc.o)
    0x00014e60   0x00014e60   0x0000002c   Code   RO         2516    i.drv_vidc_init_module_enable  CVWL668.lib(drv_vidc.o)
    0x00014e8c   0x00014e8c   0x0000000c   Code   RO         2517    i.drv_vidc_register_callback  CVWL668.lib(drv_vidc.o)
    0x00014e98   0x00014e98   0x0000000c   Code   RO         2518    i.drv_vidc_reset    CVWL668.lib(drv_vidc.o)
    0x00014ea4   0x00014ea4   0x0000001c   Code   RO         2519    i.drv_vidc_set_circ_mode_enable  CVWL668.lib(drv_vidc.o)
    0x00014ec0   0x00014ec0   0x00000038   Code   RO         2520    i.drv_vidc_set_dither_config  CVWL668.lib(drv_vidc.o)
    0x00014ef8   0x00014ef8   0x0000005c   Code   RO         2522    i.drv_vidc_set_dst_parameter  CVWL668.lib(drv_vidc.o)
    0x00014f54   0x00014f54   0x0000000c   Code   RO         2524    i.drv_vidc_set_honly_hcoef0  CVWL668.lib(drv_vidc.o)
    0x00014f60   0x00014f60   0x0000002c   Code   RO         2525    i.drv_vidc_set_honly_hinitb  CVWL668.lib(drv_vidc.o)
    0x00014f8c   0x00014f8c   0x00000030   Code   RO         2526    i.drv_vidc_set_honly_hinitr  CVWL668.lib(drv_vidc.o)
    0x00014fbc   0x00014fbc   0x0000001c   Code   RO         2529    i.drv_vidc_set_irqen  CVWL668.lib(drv_vidc.o)
    0x00014fd8   0x00014fd8   0x00000014   Code   RO         2530    i.drv_vidc_set_mirror  CVWL668.lib(drv_vidc.o)
    0x00014fec   0x00014fec   0x0000001c   Code   RO         2533    i.drv_vidc_set_pentile_swap  CVWL668.lib(drv_vidc.o)
    0x00015008   0x00015008   0x0000000c   Code   RO         2534    i.drv_vidc_set_pu_ctrl  CVWL668.lib(drv_vidc.o)
    0x00015014   0x00015014   0x00000018   Code   RO         2535    i.drv_vidc_set_rotation  CVWL668.lib(drv_vidc.o)
    0x0001502c   0x0001502c   0x0000000c   Code   RO         2536    i.drv_vidc_set_scld_hcoef0  CVWL668.lib(drv_vidc.o)
    0x00015038   0x00015038   0x0000000c   Code   RO         2537    i.drv_vidc_set_scld_hcoef1  CVWL668.lib(drv_vidc.o)
    0x00015044   0x00015044   0x00000014   Code   RO         2538    i.drv_vidc_set_scld_step  CVWL668.lib(drv_vidc.o)
    0x00015058   0x00015058   0x0000000c   Code   RO         2539    i.drv_vidc_set_scld_vcoef0  CVWL668.lib(drv_vidc.o)
    0x00015064   0x00015064   0x0000000c   Code   RO         2540    i.drv_vidc_set_scld_vcoef1  CVWL668.lib(drv_vidc.o)
    0x00015070   0x00015070   0x00000020   Code   RO         2541    i.drv_vidc_set_src_parameter  CVWL668.lib(drv_vidc.o)
    0x00015090   0x00015090   0x00000038   Code   RO         2542    i.drv_vidc_set_vintp_config  CVWL668.lib(drv_vidc.o)
    0x000150c8   0x000150c8   0x00000010   Code   RO         1931    i.drv_wdg_clear_counter  CVWL668.lib(drv_wdg.o)
    0x000150d8   0x000150d8   0x00000010   Code   RO         1932    i.drv_wdg_clear_edge_flag  CVWL668.lib(drv_wdg.o)
    0x000150e8   0x000150e8   0x00000010   Code   RO         1935    i.drv_wdg_read_edge_flag  CVWL668.lib(drv_wdg.o)
    0x000150f8   0x000150f8   0x00000034   Code   RO         1938    i.drv_wdg_set_int   CVWL668.lib(drv_wdg.o)
    0x0001512c   0x0001512c   0x00000034   Code   RO         1304    i.fputc             CVWL668.lib(tau_log.o)
    0x00015160   0x00015160   0x00000040   Code   RO         1444    i.ha_intl_fb_check_pu_size  CVWL668.lib(hal_internal_fb.o)
    0x000151a0   0x000151a0   0x00000038   Code   RO          887    i.hal_dsi_rx_ctrl_create_handle  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x000151d8   0x000151d8   0x00000040   Code   RO          888    i.hal_dsi_rx_ctrl_dcs_async_handler  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015218   0x00015218   0x00000094   Code   RO          889    i.hal_dsi_rx_ctrl_deinit  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x000152ac   0x000152ac   0x00000094   Code   RO          895    i.hal_dsi_rx_ctrl_init  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015340   0x00015340   0x00000100   Code   RO          896    i.hal_dsi_rx_ctrl_init_clk  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015440   0x00015440   0x000000f8   Code   RO          897    i.hal_dsi_rx_ctrl_init_dsi_rx  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015538   0x00015538   0x0000012c   Code   RO          898    i.hal_dsi_rx_ctrl_init_memc  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015664   0x00015664   0x00000140   Code   RO          899    i.hal_dsi_rx_ctrl_init_rxbr  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x000157a4   0x000157a4   0x0000023c   Code   RO          900    i.hal_dsi_rx_ctrl_init_vidc  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x000159e0   0x000159e0   0x00000038   Code   RO          901    i.hal_dsi_rx_ctrl_pre_init_pps  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015a18   0x00015a18   0x000000b0   Code   RO          907    i.hal_dsi_rx_ctrl_set_auto_ack  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015ac8   0x00015ac8   0x00000030   Code   RO          912    i.hal_dsi_rx_ctrl_set_ipi_cfg  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015af8   0x00015af8   0x00000030   Code   RO          917    i.hal_dsi_rx_ctrl_start  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015b28   0x00015b28   0x00000030   Code   RO          918    i.hal_dsi_rx_ctrl_stop  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015b58   0x00015b58   0x00000020   Code   RO          920    i.hal_dsi_rx_ctrl_toggle_resolution  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015b78   0x00015b78   0x0000027c   Code   RO          967    i.hal_dsi_tx_cmd_mode_cal_timing  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00015df4   0x00015df4   0x00000038   Code   RO          969    i.hal_dsi_tx_ctrl_create_handle  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00015e2c   0x00015e2c   0x00000060   Code   RO          970    i.hal_dsi_tx_ctrl_deinit  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00015e8c   0x00015e8c   0x00000022   Code   RO          972    i.hal_dsi_tx_ctrl_gen_a_tear_signal  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00015eae   0x00015eae   0x00000002   PAD
    0x00015eb0   0x00015eb0   0x00000074   Code   RO          973    i.hal_dsi_tx_ctrl_init  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00015f24   0x00015f24   0x00000010   Code   RO          974    i.hal_dsi_tx_ctrl_init_clk  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00015f34   0x00015f34   0x00000008   Code   RO          986    i.hal_dsi_tx_ctrl_set_overwrite_rgb  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00015f3c   0x00015f3c   0x0000000a   Code   RO          987    i.hal_dsi_tx_ctrl_set_tear_mode  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00015f46   0x00015f46   0x00000002   PAD
    0x00015f48   0x00015f48   0x00000070   Code   RO          989    i.hal_dsi_tx_ctrl_start  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00015fb8   0x00015fb8   0x00000038   Code   RO          990    i.hal_dsi_tx_ctrl_stop  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00015ff0   0x00015ff0   0x000000f4   Code   RO          992    i.hal_dsi_tx_ctrl_write_array_cmd  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000160e4   0x000160e4   0x000000d0   Code   RO          993    i.hal_dsi_tx_ctrl_write_cmd  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000161b4   0x000161b4   0x0000010c   Code   RO          994    i.hal_dsi_tx_init_cfg  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000162c0   0x000162c0   0x00000038   Code   RO          995    i.hal_dsi_tx_init_dpi_timing  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000162f8   0x000162f8   0x00000016   Code   RO          996    i.hal_dsi_tx_init_phy_cfg  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x0001630e   0x0001630e   0x00000052   Code   RO          997    i.hal_dsi_tx_init_timing  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00016360   0x00016360   0x00000054   Code   RO          998    i.hal_dsi_tx_init_vid_timing  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000163b4   0x000163b4   0x00000038   Code   RO          999    i.hal_dsi_tx_send_cmd  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000163ec   0x000163ec   0x00000084   Code   RO         1000    i.hal_dsi_tx_timing_info_update  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00016470   0x00016470   0x00000310   Code   RO         1001    i.hal_dsi_tx_vid_mode_cal_timing  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00016780   0x00016780   0x0000003a   Code   RO         1064    i.hal_gpio_config_pad  CVWL668.lib(hal_gpio.o)
    0x000167ba   0x000167ba   0x00000002   PAD
    0x000167bc   0x000167bc   0x00000018   Code   RO         1065    i.hal_gpio_ctrl_eint  CVWL668.lib(hal_gpio.o)
    0x000167d4   0x000167d4   0x00000040   Code   RO         1069    i.hal_gpio_init_eint  CVWL668.lib(hal_gpio.o)
    0x00016814   0x00016814   0x00000024   Code   RO         1070    i.hal_gpio_init_input  CVWL668.lib(hal_gpio.o)
    0x00016838   0x00016838   0x00000028   Code   RO         1071    i.hal_gpio_init_output  CVWL668.lib(hal_gpio.o)
    0x00016860   0x00016860   0x00000018   Code   RO         1072    i.hal_gpio_reg_eint_cb  CVWL668.lib(hal_gpio.o)
    0x00016878   0x00016878   0x00000050   Code   RO         1073    i.hal_gpio_set_ap_reset_int  CVWL668.lib(hal_gpio.o)
    0x000168c8   0x000168c8   0x00000064   Code   RO         1076    i.hal_gpio_set_mode  CVWL668.lib(hal_gpio.o)
    0x0001692c   0x0001692c   0x00000008   Code   RO         1077    i.hal_gpio_set_output_data  CVWL668.lib(hal_gpio.o)
    0x00016934   0x00016934   0x00000048   Code   RO         1078    i.hal_gpio_set_pull_state  CVWL668.lib(hal_gpio.o)
    0x0001697c   0x0001697c   0x00000010   Code   RO         1356    i.hal_internal_sync_get_hight_performan_mode  CVWL668.lib(hal_internal_vsync.o)
    0x0001698c   0x0001698c   0x000001b0   Code   RO         1357    i.hal_internal_sync_input_resolution_change  CVWL668.lib(hal_internal_vsync.o)
    0x00016b3c   0x00016b3c   0x0000000c   Code   RO         1358    i.hal_internal_sync_register_lcdc_cb  CVWL668.lib(hal_internal_vsync.o)
    0x00016b48   0x00016b48   0x00000020   Code   RO         1361    i.hal_internal_vsync_deinit  CVWL668.lib(hal_internal_vsync.o)
    0x00016b68   0x00016b68   0x0000000c   Code   RO         1362    i.hal_internal_vsync_get_rx_state  CVWL668.lib(hal_internal_vsync.o)
    0x00016b74   0x00016b74   0x00000018   Code   RO         1363    i.hal_internal_vsync_get_sync_line  CVWL668.lib(hal_internal_vsync.o)
    0x00016b8c   0x00016b8c   0x0000000c   Code   RO         1364    i.hal_internal_vsync_get_tx_state  CVWL668.lib(hal_internal_vsync.o)
    0x00016b98   0x00016b98   0x000000d8   Code   RO         1365    i.hal_internal_vsync_init_rx  CVWL668.lib(hal_internal_vsync.o)
    0x00016c70   0x00016c70   0x000000c4   Code   RO         1366    i.hal_internal_vsync_init_tx  CVWL668.lib(hal_internal_vsync.o)
    0x00016d34   0x00016d34   0x00000020   Code   RO         1367    i.hal_internal_vsync_set_rx_state  CVWL668.lib(hal_internal_vsync.o)
    0x00016d54   0x00016d54   0x000000f8   Code   RO         1369    i.hal_internal_vsync_set_tear_mode  CVWL668.lib(hal_internal_vsync.o)
    0x00016e4c   0x00016e4c   0x0000006c   Code   RO         1370    i.hal_internal_vsync_set_tx_state  CVWL668.lib(hal_internal_vsync.o)
    0x00016eb8   0x00016eb8   0x0000006c   Code   RO         1417    i.hal_intl_dcs_init_sw_fltr  CVWL668.lib(hal_internal_dcs.o)
    0x00016f24   0x00016f24   0x0000044c   Code   RO         1419    i.hal_intl_dcs_rx_get_dcs_packet_data  CVWL668.lib(hal_internal_dcs.o)
    0x00017370   0x00017370   0x00000088   Code   RO         1420    i.hal_intl_dcs_rx_receive_packet  CVWL668.lib(hal_internal_dcs.o)
    0x000173f8   0x000173f8   0x00000174   Code   RO         1421    i.hal_intl_dcs_rx_receive_pps  CVWL668.lib(hal_internal_dcs.o)
    0x0001756c   0x0001756c   0x0000008c   Code   RO         1422    i.hal_intl_dcs_set_auto_hw_filter  CVWL668.lib(hal_internal_dcs.o)
    0x000175f8   0x000175f8   0x0000002c   Code   RO         1424    i.hal_intl_dcs_sw_filter_handle  CVWL668.lib(hal_internal_dcs.o)
    0x00017624   0x00017624   0x000002e0   Code   RO         1445    i.hal_intl_fb_cal_fb_info  CVWL668.lib(hal_internal_fb.o)
    0x00017904   0x00017904   0x00000064   Code   RO         1446    i.hal_intl_fb_check_bandwidth  CVWL668.lib(hal_internal_fb.o)
    0x00017968   0x00017968   0x000000c8   Code   RO         1447    i.hal_intl_fb_edge_resize  CVWL668.lib(hal_internal_fb.o)
    0x00017a30   0x00017a30   0x00000064   Code   RO         1448    i.hal_intl_fb_flow_control_adapter  CVWL668.lib(hal_internal_fb.o)
    0x00017a94   0x00017a94   0x0000000c   Code   RO         1449    i.hal_intl_fb_get_memc_flow_mode  CVWL668.lib(hal_internal_fb.o)
    0x00017aa0   0x00017aa0   0x00000010   Code   RO         1450    i.hal_intl_fb_get_rx_fb_info  CVWL668.lib(hal_internal_fb.o)
    0x00017ab0   0x00017ab0   0x00000010   Code   RO         1451    i.hal_intl_fb_get_tx_fb_info  CVWL668.lib(hal_internal_fb.o)
    0x00017ac0   0x00017ac0   0x0000000c   Code   RO         1452    i.hal_intl_fb_get_user_flow  CVWL668.lib(hal_internal_fb.o)
    0x00017acc   0x00017acc   0x00000028   Code   RO         1470    i.hal_intl_svs_deinit_rx  CVWL668.lib(hal_internal_svs.o)
    0x00017af4   0x00017af4   0x00000010   Code   RO         1471    i.hal_intl_svs_deinit_tx  CVWL668.lib(hal_internal_svs.o)
    0x00017b04   0x00017b04   0x00000024   Code   RO         1472    i.hal_intl_svs_handle  CVWL668.lib(hal_internal_svs.o)
    0x00017b28   0x00017b28   0x00000080   Code   RO         1473    i.hal_intl_svs_init_rx  CVWL668.lib(hal_internal_svs.o)
    0x00017ba8   0x00017ba8   0x00000014   Code   RO         1474    i.hal_intl_svs_init_tx  CVWL668.lib(hal_internal_svs.o)
    0x00017bbc   0x00017bbc   0x0000000c   Code   RO         1476    i.hal_intl_svs_set_rx_vtt  CVWL668.lib(hal_internal_svs.o)
    0x00017bc8   0x00017bc8   0x00000048   Code   RO         1478    i.hal_intl_svs_update_rxbr_clk  CVWL668.lib(hal_internal_svs.o)
    0x00017c10   0x00017c10   0x00000070   Code   RO         1002    i.hal_lcdc_displayproc_config  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00017c80   0x00017c80   0x00000064   Code   RO         1003    i.hal_lcdc_func_update  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00017ce4   0x00017ce4   0x0000003e   Code   RO         1004    i.hal_lcdc_init_cfg  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00017d22   0x00017d22   0x00000070   Code   RO         1005    i.hal_lcdc_init_clk  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00017d92   0x00017d92   0x00000002   PAD
    0x00017d94   0x00017d94   0x00000128   Code   RO         1006    i.hal_lcdc_postproc_config  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00017ebc   0x00017ebc   0x00000024   Code   RO         1007    i.hal_lcdc_start    CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00017ee0   0x00017ee0   0x0000003c   Code   RO         1008    i.hal_lcdc_timinggen_config  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00017f1c   0x00017f1c   0x000000d4   Code   RO         1009    i.hal_lcdc_upscaler_config  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00017ff0   0x00017ff0   0x0000002a   Code   RO         1257    i.hal_pwr_enter_deep_sleep_mode  CVWL668.lib(hal_pwr.o)
    0x0001801a   0x0001801a   0x00000008   Code   RO         1258    i.hal_pwr_enter_normal_sleep_mode  CVWL668.lib(hal_pwr.o)
    0x00018022   0x00018022   0x00000002   PAD
    0x00018024   0x00018024   0x00000064   Code   RO         1259    i.hal_pwr_enter_stop_sleep_mode  CVWL668.lib(hal_pwr.o)
    0x00018088   0x00018088   0x0000000a   Code   RO         1260    i.hal_pwr_exit_sleep_mode  CVWL668.lib(hal_pwr.o)
    0x00018092   0x00018092   0x00000008   Code   RO         1262    i.hal_pwr_get_vcc_power_ready  CVWL668.lib(hal_pwr.o)
    0x0001809a   0x0001809a   0x00000008   Code   RO         1267    i.hal_pwr_set_main_power  CVWL668.lib(hal_pwr.o)
    0x000180a2   0x000180a2   0x00000008   Code   RO         1268    i.hal_pwr_set_sleep_mode_power  CVWL668.lib(hal_pwr.o)
    0x000180aa   0x000180aa   0x00000002   PAD
    0x000180ac   0x000180ac   0x00000064   Code   RO         1269    i.hal_pwr_set_stop_sleep_wakeup_pin  CVWL668.lib(hal_pwr.o)
    0x00018110   0x00018110   0x00000040   Code   RO         1156    i.hal_swire_deinit  CVWL668.lib(hal_swire.o)
    0x00018150   0x00018150   0x0000005c   Code   RO         1157    i.hal_swire_enable  CVWL668.lib(hal_swire.o)
    0x000181ac   0x000181ac   0x00000058   Code   RO         1158    i.hal_swire_init    CVWL668.lib(hal_swire.o)
    0x00018204   0x00018204   0x00000024   Code   RO         1160    i.hal_swire_set_pulse  CVWL668.lib(hal_swire.o)
    0x00018228   0x00018228   0x00000040   Code   RO         1161    i.hal_swire_set_timer  CVWL668.lib(hal_swire.o)
    0x00018268   0x00018268   0x00000118   Code   RO         1181    i.hal_system_init   CVWL668.lib(hal_system.o)
    0x00018380   0x00018380   0x00000030   Code   RO         1197    i.hal_timer_deinit  CVWL668.lib(hal_timer.o)
    0x000183b0   0x000183b0   0x0000001c   Code   RO         1199    i.hal_timer_init    CVWL668.lib(hal_timer.o)
    0x000183cc   0x000183cc   0x00000008   Code   RO         1200    i.hal_timer_set_repeat  CVWL668.lib(hal_timer.o)
    0x000183d4   0x000183d4   0x00000030   Code   RO         1201    i.hal_timer_start   CVWL668.lib(hal_timer.o)
    0x00018404   0x00018404   0x00000028   Code   RO         1203    i.hal_timer_stop    CVWL668.lib(hal_timer.o)
    0x0001842c   0x0001842c   0x00000030   Code   RO         1010    i.hal_tx_frame_rate_adjust  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x0001845c   0x0001845c   0x00000094   Code   RO         1328    i.hal_uart_init     CVWL668.lib(hal_uart.o)
    0x000184f0   0x000184f0   0x0000001c   Code   RO         1331    i.hal_uart_send_blocking  CVWL668.lib(hal_uart.o)
    0x0001850c   0x0001850c   0x000000cc   Code   RO         1372    i.hal_vsync_reset_lcdc_scaler  CVWL668.lib(hal_internal_vsync.o)
    0x000185d8   0x000185d8   0x00000040   Code   RO            3    i.main              main.o
    0x00018618   0x00018618   0x00000054   Code   RO          344    i.pps_update_handle  s8_demo.o
    0x0001866c   0x0001866c   0x000002ac   Code   RO         1373    i.rxbr_irq1_callback  CVWL668.lib(hal_internal_vsync.o)
    0x00018918   0x00018918   0x00000060   Code   RO          345    i.s8_demo           s8_demo.o
    0x00018978   0x00018978   0x0000003a   Code   RO          346    i.send_panel_init_code  s8_demo.o
    0x000189b2   0x000189b2   0x00000002   PAD
    0x000189b4   0x000189b4   0x00000044   Code   RO         1374    i.soft_double_buffer_update  CVWL668.lib(hal_internal_vsync.o)
    0x000189f8   0x000189f8   0x00000044   Code   RO         1375    i.soft_gen_te       CVWL668.lib(hal_internal_vsync.o)
    0x00018a3c   0x00018a3c   0x00000054   Code   RO         1376    i.soft_gen_te_double_buffer  CVWL668.lib(hal_internal_vsync.o)
    0x00018a90   0x00018a90   0x00000038   Code   RO          347    i.soft_swire_init   s8_demo.o
    0x00018ac8   0x00018ac8   0x0000002e   Code   RO          348    i.soft_swire_start  s8_demo.o
    0x00018af6   0x00018af6   0x00000002   PAD
    0x00018af8   0x00018af8   0x00000048   Code   RO          349    i.soft_swire_timer_callback  s8_demo.o
    0x00018b40   0x00018b40   0x00000018   Code   RO         1271    i.stop_sleep_cb     CVWL668.lib(hal_pwr.o)
    0x00018b58   0x00018b58   0x000000ac   Code   RO         1479    i.svs_direct_mode_setting  CVWL668.lib(hal_internal_svs.o)
    0x00018c04   0x00018c04   0x0000001c   Code   RO         1480    i.svs_get_rel_intv  CVWL668.lib(hal_internal_svs.o)
    0x00018c20   0x00018c20   0x000000b0   Code   RO         1481    i.svs_sync_handle   CVWL668.lib(hal_internal_svs.o)
    0x00018cd0   0x00018cd0   0x000000cc   Code   RO         1482    i.svs_wait_fr_stab  CVWL668.lib(hal_internal_svs.o)
    0x00018d9c   0x00018d9c   0x0000010c   Code   RO         1483    i.svs_wait_start    CVWL668.lib(hal_internal_svs.o)
    0x00018ea8   0x00018ea8   0x00000034   Code   RO         1305    i.tau_log_init      CVWL668.lib(tau_log.o)
    0x00018edc   0x00018edc   0x00000084   Code   RO         1306    i.tau_log_printf    CVWL668.lib(tau_log.o)
    0x00018f60   0x00018f60   0x00000076   Code   RO         1307    i.tau_log_push_log  CVWL668.lib(tau_log.o)
    0x00018fd6   0x00018fd6   0x00000002   PAD
    0x00018fd8   0x00018fd8   0x000000b4   Code   RO         1377    i.vidc_callback     CVWL668.lib(hal_internal_vsync.o)
    0x0001908c   0x0001908c   0x00000130   Code   RO         1378    i.vpre_err_reset    CVWL668.lib(hal_internal_vsync.o)
    0x000191bc   0x000191bc   0x00001efc   Data   RO          350    .constdata          s8_demo.o
    0x0001b0b8   0x0001b0b8   0x00000028   Data   RO          922    .constdata          CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x0001b0e0   0x0001b0e0   0x0000001c   Data   RO         1013    .constdata          CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x0001b0fc   0x0001b0fc   0x000000d0   Data   RO         1081    .constdata          CVWL668.lib(hal_gpio.o)
    0x0001b1cc   0x0001b1cc   0x00000030   Data   RO         1333    .constdata          CVWL668.lib(hal_uart.o)
    0x0001b1fc   0x0001b1fc   0x00000010   Data   RO         2609    .constdata          CVWL668.lib(drv_uart.o)
    0x0001b20c   0x0001b20c   0x00000087   Data   RO          923    .conststring        CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x0001b293   0x0001b293   0x00000001   PAD
    0x0001b294   0x0001b294   0x0000008e   Data   RO         1380    .conststring        CVWL668.lib(hal_internal_vsync.o)
    0x0001b322   0x0001b322   0x00000002   PAD
    0x0001b324   0x0001b324   0x0000008e   Data   RO         1427    .conststring        CVWL668.lib(hal_internal_dcs.o)
    0x0001b3b2   0x0001b3b2   0x00000002   PAD
    0x0001b3b4   0x0001b3b4   0x00000020   Data   RO         3009    Region$$Table       anon$$obj.o


    Execution Region RW_IRAM1 (Exec base: 0x00070000, Load base: 0x0001b3d4, Size: 0x000030e8, Max: 0x00008000, ABSOLUTE, COMPRESSED[0x00000164])

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00070000   COMPRESSED   0x0000008e   Data   RW          351    .data               s8_demo.o
    0x0007008e   COMPRESSED   0x00000002   PAD
    0x00070090   COMPRESSED   0x00000008   Data   RW          924    .data               CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00070098   COMPRESSED   0x0000005c   Data   RW         1014    .data               CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000700f4   COMPRESSED   0x00000001   Data   RW         1142    .data               CVWL668.lib(hal_spi_master.o)
    0x000700f5   COMPRESSED   0x00000002   Data   RW         1163    .data               CVWL668.lib(hal_swire.o)
    0x000700f7   COMPRESSED   0x00000001   PAD
    0x000700f8   COMPRESSED   0x00000008   Data   RW         1272    .data               CVWL668.lib(hal_pwr.o)
    0x00070100   COMPRESSED   0x00000001   Data   RW         1310    .data               CVWL668.lib(tau_log.o)
    0x00070101   COMPRESSED   0x00000003   PAD
    0x00070104   COMPRESSED   0x00000018   Data   RW         1334    .data               CVWL668.lib(hal_uart.o)
    0x0007011c   COMPRESSED   0x00000008   Data   RW         1381    .data               CVWL668.lib(hal_internal_vsync.o)
    0x00070124   COMPRESSED   0x00000024   Data   RW         1428    .data               CVWL668.lib(hal_internal_dcs.o)
    0x00070148   COMPRESSED   0x0000000c   Data   RW         1512    .data               CVWL668.lib(drv_common.o)
    0x00070154   COMPRESSED   0x00000001   Data   RW         1513    .data               CVWL668.lib(drv_common.o)
    0x00070155   COMPRESSED   0x00000003   PAD
    0x00070158   COMPRESSED   0x00000190   Data   RW         1598    .data               CVWL668.lib(drv_dma.o)
    0x000702e8   COMPRESSED   0x00000004   Data   RW         1660    .data               CVWL668.lib(drv_gpio.o)
    0x000702ec   COMPRESSED   0x00000004   Data   RW         1845    .data               CVWL668.lib(drv_swire.o)
    0x000702f0   COMPRESSED   0x00000050   Data   RW         1911    .data               CVWL668.lib(drv_timer.o)
    0x00070340   COMPRESSED   0x0000000c   Data   RW         1940    .data               CVWL668.lib(drv_wdg.o)
    0x0007034c   COMPRESSED   0x0000003c   Data   RW         2026    .data               CVWL668.lib(drv_i2c.o)
    0x00070388   COMPRESSED   0x00000004   Data   RW         2084    .data               CVWL668.lib(drv_se.o)
    0x0007038c   COMPRESSED   0x00000001   Data   RW         2124    .data               CVWL668.lib(drv_dsi_rx.o)
    0x0007038d   COMPRESSED   0x00000003   PAD
    0x00070390   COMPRESSED   0x00000008   Data   RW         2458    .data               CVWL668.lib(drv_rxbr.o)
    0x00070398   COMPRESSED   0x00000004   Data   RW         2544    .data               CVWL668.lib(drv_vidc.o)
    0x0007039c   COMPRESSED   0x00000004   Data   RW         2987    .data               mc_p.l(stdout.o)
    0x000703a0        -       0x000000cc   Zero   RW          921    .bss                CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x0007046c        -       0x000000b4   Zero   RW         1012    .bss                CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00070520        -       0x00000100   Zero   RW         1309    .bss                CVWL668.lib(tau_log.o)
    0x00070620        -       0x00000024   Zero   RW         1379    .bss                CVWL668.lib(hal_internal_vsync.o)
    0x00070644        -       0x00000800   Zero   RW         1425    .bss                CVWL668.lib(hal_internal_dcs.o)
    0x00070e44        -       0x000000ff   Zero   RW         1426    .bss                CVWL668.lib(hal_internal_dcs.o)
    0x00070f43   COMPRESSED   0x00000001   PAD
    0x00070f44        -       0x00000044   Zero   RW         1454    .bss                CVWL668.lib(hal_internal_fb.o)
    0x00070f88        -       0x00000044   Zero   RW         1484    .bss                CVWL668.lib(hal_internal_svs.o)
    0x00070fcc        -       0x00000010   Zero   RW         1596    .bss                CVWL668.lib(drv_dma.o)
    0x00070fdc        -       0x00000040   Zero   RW         1659    .bss                CVWL668.lib(drv_gpio.o)
    0x0007101c        -       0x0000106c   Zero   RW         2067    .bss                CVWL668.lib(dcs_packet_fifo.o)
    0x00072088        -       0x00000060   Zero   RW         2608    .bss                CVWL668.lib(drv_uart.o)
    0x000720e8        -       0x00001000   Zero   RW          536    STACK               startup_armcm0.o


==============================================================================

Image component sizes


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Object Name

         0          0          0          0          0       5016   app_tp_transfer.o
        44          6          0          0          0        461   board.o
        64         32          0          0          0      10227   main.o
      2522        598       7932        142          0      22509   s8_demo.o
       120         18        192          0       4096       2044   startup_armcm0.o

    ----------------------------------------------------------------------
      2756        654       8156        144       4096      40257   Object Totals
         0          0         32          0          0          0   (incl. Generated)
         6          0          0          2          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Member Name

       216         32          0          0       4204        252   dcs_packet_fifo.o
       104         62         28         13          0        192   drv_common.o
       536         90          0          0          0        792   drv_crgu.o
       136         22          0        400         16        196   drv_dma.o
       120         34          0          0          0        188   drv_dsc_dec.o
      1788        662          0          1          0       1280   drv_dsi_rx.o
      1704        306          0          0          0       2036   drv_dsi_tx.o
       148          0          0          0          0        260   drv_efuse.o
       340         50          0          4         64       1132   drv_gpio.o
        36         12          0         60          0        180   drv_i2c.o
      1080        166          0          0          0       1620   drv_lcdc.o
       658        104          0          0          0       1240   drv_memc.o
        40          0          0          0          0        120   drv_phy_common.o
       556        122          0          0          0        708   drv_pwr.o
       814        110          0          8          0       1136   drv_rxbr.o
      1012        264          0          4          0        492   drv_se.o
       116         32          0          0          0        308   drv_spi_master.o
       264         54          0          4          0        560   drv_swire.o
       220         40          0          0          0        428   drv_sys_cfg.o
       386         44          0         80          0        876   drv_timer.o
      1172         54         16          0         96        980   drv_uart.o
       824        152          0          4          0       1700   drv_vidc.o
       156         22          0         12          0        316   drv_wdg.o
      2546        194        175          8        204       1168   hal_dsi_rx_ctrl.o
      4114        318         50         92        180       2140   hal_dsi_tx_ctrl.o
       538         42        208          0          0        760   hal_gpio.o
      2168        508        142         36       2303        652   hal_internal_dcs.o
      1256         58          0          0         68        688   hal_internal_fb.o
      1172        182          0          0         68        840   hal_internal_svs.o
      3232        748        142          8         36       1556   hal_internal_vsync.o
       308         32          0          8          0        616   hal_pwr.o
        64          4          0          1          0         68   hal_spi_master.o
       344         32          0          2          0        348   hal_swire.o
       280         56          0          0          0         72   hal_system.o
       172          0          0          0          0        344   hal_timer.o
       176         18         48         24          0        144   hal_uart.o
        68          4          0          0          0        136   tau_delay.o
       354         30         16          1        256        320   tau_log.o
       200         20          0          0          0         76   ceil.o
        86          0          0          0          0          0   __dczerorl2.o
         0          0          0          0          0          0   entry.o
         0          0          0          0          0          0   entry10a.o
         0          0          0          0          0          0   entry11a.o
         8          4          0          0          0          0   entry2.o
         4          0          0          0          0          0   entry5.o
         0          0          0          0          0          0   entry7b.o
         0          0          0          0          0          0   entry8b.o
         8          4          0          0          0          0   entry9a.o
        30          0          0          0          0          0   handlers.o
        40          0          0          0          0         72   idiv.o
        36          8          0          0          0         68   init.o
         0          0          0          0          0          0   iusefp.o
        32          0          0          0          0         68   llshl.o
        38          0          0          0          0         68   llsshr.o
        34          0          0          0          0         68   llushr.o
        36          0          0          0          0         60   memcpya.o
        36          0          0          0          0        100   memseta.o
      2298        104          0          0          0        544   printfa.o
         0          0          0          4          0          0   stdout.o
        14          0          0          0          0         60   strlen.o
        44          0          0          0          0         72   uidiv.o
        96          0          0          0          0         84   uldiv.o
        40          2          0          0          0         68   cdrcmple.o
        20          0          0          0          0         68   cfcmple.o
        20          0          0          0          0         68   cfrcmple.o
        56          0          0          0          0         68   d2f.o
       356          4          0          0          0        140   dadd.o
       240          6          0          0          0         84   ddiv.o
       236          0          0          0          0        216   depilogue.o
        60         10          0          0          0         68   dfixui.o
        64         10          0          0          0         68   dfixul.o
        28          4          0          0          0         68   dfltui.o
       208          6          0          0          0         88   dmul.o
        40          0          0          0          0         60   f2d.o
       178          0          0          0          0        108   fadd.o
       124          0          0          0          0         72   fdiv.o
       130          0          0          0          0        144   fepilogue.o
        40          0          0          0          0         60   ffixui.o
        14          0          0          0          0         68   ffltui.o
       122          0          0          0          0         72   fmul.o
        24          0          0          0          0         60   fscalb.o

    ----------------------------------------------------------------------
     34292       4842        832        784       7496      29832   Library Totals
        34          0          7         10          1          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Name

     29218       4660        825        770       7495      26844   CVWL668.lib
       200         20          0          0          0         76   m_ps.l
      2840        120          0          4          0       1264   mc_p.l
      2000         42          0          0          0       1648   mf_p.l

    ----------------------------------------------------------------------
     34292       4842        832        784       7496      29832   Library Totals

    ----------------------------------------------------------------------

==============================================================================


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   

     37048       5496       8988        928      11592      50005   Grand Totals
     37048       5496       8988        356      11592      50005   ELF Image Totals (compressed)
     37048       5496       8988        356          0          0   ROM Totals

==============================================================================

    Total RO  Size (Code + RO Data)                46036 (  44.96kB)
    Total RW  Size (RW Data + ZI Data)             12520 (  12.23kB)
    Total ROM Size (Code + RO Data + RW Data)      46392 (  45.30kB)

==============================================================================

