Component: ARM Compiler 5.06 update 6 (build 750) Tool: armlink [4d35ed]

==============================================================================

Section Cross References

    main.o(i.main) refers to board.o(i.board_Init) for board_Init
    main.o(i.main) refers to s8_demo.o(i.s8_demo) for s8_demo
    main.o(i.main) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(i.app_tp_transfer_phone) for app_tp_transfer_phone
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(i.app_tp_s_write) for app_tp_s_write
    app_tp_transfer.o(i.app_tp_i2cs_callback) refers to app_tp_transfer.o(.data) for i2cs_transfer
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(i.app_tp_phone_reset_init) for app_tp_phone_reset_init
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(i.app_tp_screen_int_init) for app_tp_screen_int_init
    app_tp_transfer.o(i.app_tp_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(i.screen_spim_io_init) for screen_spim_io_init
    app_tp_transfer.o(i.app_tp_init) refers to hal_spi_master.o(i.hal_spim_init) for hal_spim_init
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(i.phone_i2cs_io_init) for phone_i2cs_io_init
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_slave.o(i.hal_i2cs_init) for hal_i2cs_init
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_slave.o(i.hal_i2cs_register_callback) for hal_i2cs_register_callback
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) for hal_i2cs_update_rx_buffer
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer) for hal_i2cs_update_tx_buffer
    app_tp_transfer.o(i.app_tp_init) refers to hal_i2c_slave.o(i.hal_i2cs_start) for hal_i2cs_start
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_for_custom_s8.o(.data) for g_phone_output_int_pad
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(i.app_tp_i2cs_callback) for app_tp_i2cs_callback
    app_tp_transfer.o(i.app_tp_init) refers to app_tp_transfer.o(.bss) for s_phone_read_buffer
    app_tp_transfer.o(i.app_tp_m_read) refers to hal_spi_master.o(i.hal_spim_read) for hal_spim_read
    app_tp_transfer.o(i.app_tp_m_transfer_complate) refers to hal_spi_master.o(i.hal_spim_get_transfer_complete) for hal_spim_get_transfer_complete
    app_tp_transfer.o(i.app_tp_m_write) refers to hal_spi_master.o(i.hal_spim_write) for hal_spim_write
    app_tp_transfer.o(i.app_tp_m_write) refers to app_tp_transfer.o(.data) for s_spim_write
    app_tp_transfer.o(i.app_tp_phone_clear_reset_on) refers to app_tp_transfer.o(.data) for s_phone_reset_flag
    app_tp_transfer.o(i.app_tp_phone_reset_init) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    app_tp_transfer.o(i.app_tp_phone_reset_init) refers to hal_gpio.o(i.hal_gpio_ctrl_eint) for hal_gpio_ctrl_eint
    app_tp_transfer.o(i.app_tp_phone_reset_init) refers to hal_gpio.o(i.hal_gpio_init_eint) for hal_gpio_init_eint
    app_tp_transfer.o(i.app_tp_phone_reset_init) refers to hal_gpio.o(i.hal_gpio_reg_eint_cb) for hal_gpio_reg_eint_cb
    app_tp_transfer.o(i.app_tp_phone_reset_init) refers to app_tp_for_custom_s8.o(.data) for g_phone_input_rst_pad
    app_tp_transfer.o(i.app_tp_phone_reset_init) refers to app_tp_transfer.o(i.app_tp_reset_callback) for app_tp_reset_callback
    app_tp_transfer.o(i.app_tp_phone_reset_on) refers to app_tp_transfer.o(.data) for s_phone_reset_flag
    app_tp_transfer.o(i.app_tp_reset_callback) refers to app_tp_transfer.o(.data) for s_phone_reset_flag
    app_tp_transfer.o(i.app_tp_s_read) refers to hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) for hal_i2cs_update_rx_buffer
    app_tp_transfer.o(i.app_tp_s_write) refers to hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer) for hal_i2cs_update_tx_buffer
    app_tp_transfer.o(i.app_tp_screen_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    app_tp_transfer.o(i.app_tp_screen_init) refers to tau_delay.o(i.delayUs) for delayUs
    app_tp_transfer.o(i.app_tp_screen_init) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_transfer.o(i.app_tp_screen_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_rst_pad
    app_tp_transfer.o(i.app_tp_screen_int_callback) refers to app_tp_transfer.o(.data) for s_screen_int_flag
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to hal_gpio.o(i.hal_gpio_ctrl_eint) for hal_gpio_ctrl_eint
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to hal_gpio.o(i.hal_gpio_init_eint) for hal_gpio_init_eint
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to hal_gpio.o(i.hal_gpio_reg_eint_cb) for hal_gpio_reg_eint_cb
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.app_tp_screen_int_init) refers to app_tp_transfer.o(i.app_tp_screen_int_callback) for app_tp_screen_int_callback
    app_tp_transfer.o(i.app_tp_screen_int_lvl_low) refers to hal_gpio.o(i.hal_gpio_get_input_data) for hal_gpio_get_input_data
    app_tp_transfer.o(i.app_tp_screen_int_lvl_low) refers to app_tp_for_custom_s8.o(.data) for g_screen_input_int_pad
    app_tp_transfer.o(i.app_tp_transfer_phone) refers to app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) for app_tp_phone_analysis_data
    app_tp_transfer.o(i.app_tp_transfer_phone) refers to app_tp_transfer.o(i.app_tp_s_read) for app_tp_s_read
    app_tp_transfer.o(i.app_tp_transfer_phone) refers to app_tp_transfer.o(.data) for s_slave_txbuffer_size
    app_tp_transfer.o(i.app_tp_transfer_phone) refers to app_tp_transfer.o(.bss) for s_phone_read_buffer
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(i.app_tp_m_transfer_complate) for app_tp_m_transfer_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to hal_spi_master.o(i.hal_spim_flush) for hal_spim_flush
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) for app_tp_screen_analysis_const
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(.data) for s_screen_const_transfer_count
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_for_custom_s8.o(.constdata) for screen_reg_start_data_size
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_for_custom_s8.o(.data) for screen_reg_start_data
    app_tp_transfer.o(i.app_tp_transfer_screen_const) refers to app_tp_transfer.o(.bss) for s_screen_read_buffer
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_transfer_screen_const) for app_tp_transfer_screen_const
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_screen_int_lvl_low) for app_tp_screen_int_lvl_low
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_m_transfer_complate) for app_tp_m_transfer_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_spi_master.o(i.hal_spim_flush) for hal_spim_flush
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_m_write) for app_tp_m_write
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(i.app_tp_m_read) for app_tp_m_read
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) for app_tp_screen_analysis_int
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to hal_system.o(i.hal_system_get_tick) for hal_system_get_tick
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(i.app_tp_write_other_operations) for app_tp_write_other_operations
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(.data) for s_screen_init_complate
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(.data) for screen_reg_int_data
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_transfer.o(.bss) for s_screen_read_buffer
    app_tp_transfer.o(i.app_tp_transfer_screen_int) refers to app_tp_for_custom_s8.o(.constdata) for screen_reg_int_data_size
    app_tp_transfer.o(i.app_tp_transfer_screen_start) refers to app_tp_transfer.o(i.app_tp_screen_init) for app_tp_screen_init
    app_tp_transfer.o(i.app_tp_transfer_screen_start) refers to app_tp_transfer.o(i.app_tp_transfer_screen_const) for app_tp_transfer_screen_const
    app_tp_transfer.o(i.app_tp_transfer_screen_start) refers to app_tp_transfer.o(.data) for s_screen_init_complate
    app_tp_transfer.o(i.phone_i2cs_io_init) refers to hal_gpio.o(i.hal_gpio_config_pad) for hal_gpio_config_pad
    app_tp_transfer.o(i.phone_i2cs_io_init) refers to app_tp_transfer.o(.constdata) for .constdata
    app_tp_transfer.o(i.screen_spim_io_init) refers to hal_gpio.o(i.hal_gpio_config_pad) for hal_gpio_config_pad
    app_tp_transfer.o(i.screen_spim_io_init) refers to app_tp_transfer.o(.constdata) for .constdata
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to app_tp_for_custom_s8.o(.data) for start_now
    app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data) refers to app_tp_for_custom_s8.o(.constdata) for phone_60_start_back
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to app_tp_transfer.o(i.app_tp_screen_init) for app_tp_screen_init
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to tau_delay.o(i.delayMs) for delayMs
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const) refers to app_tp_for_custom_s8.o(.data) for app_tp_count
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to ffltui.o(.text) for __aeabi_ui2f
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to fmul.o(.text) for __aeabi_fmul
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to fdiv.o(.text) for __aeabi_fdiv
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to ffixui.o(.text) for __aeabi_f2uiz
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to f2d.o(.text) for __aeabi_f2d
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to dmul.o(.text) for __aeabi_dmul
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to ddiv.o(.text) for __aeabi_ddiv
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to dfixui.o(.text) for __aeabi_d2uiz
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to app_tp_for_custom_s8.o(.data) for phone_reg_coord_BUF_NUM
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to app_tp_for_custom_s8.o(.bss) for Touch
    app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_for_custom_s8.o(i.app_tp_write_other_operations) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    app_tp_for_custom_s8.o(i.app_tp_write_other_operations) refers to app_tp_for_custom_s8.o(.data) for start_now
    app_tp_for_custom_s8.o(.data) refers to app_tp_for_custom_s8.o(.constdata) for screen_87_data
    s8_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) for hal_dsi_rx_ctrl_send_ack_cmd
    s8_demo.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) for hal_dsi_rx_ctrl_get_max_ret_size
    s8_demo.o(i.ap_dcs_read) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.ap_dcs_read) refers to s8_demo.o(.data) for g_rx_ctrl_handle
    s8_demo.o(i.ap_dcs_set_backlight) refers to idiv.o(.text) for __aeabi_idivmod
    s8_demo.o(i.ap_dcs_set_backlight) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    s8_demo.o(i.ap_dcs_set_backlight) refers to s8_demo.o(.data) for AP_REG51_7FF
    s8_demo.o(i.ap_dcs_set_display_on) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    s8_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to tau_delay.o(i.delayMs) for delayMs
    s8_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    s8_demo.o(i.ap_dcs_set_enter_sleep_mode) refers to s8_demo.o(.data) for sg_system_suspend
    s8_demo.o(i.ap_dcs_set_exit_sleep_mode) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    s8_demo.o(i.ap_dcs_set_exit_sleep_mode) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.ap_dcs_set_exit_sleep_mode) refers to s8_demo.o(.data) for panel_display_done
    s8_demo.o(i.ap_dcs_set_eye_protection_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm) for hal_dsi_tx_ctrl_set_ccm
    s8_demo.o(i.ap_rstn_pull_down_cb) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    s8_demo.o(i.ap_rstn_pull_down_cb) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.ap_rstn_pull_down_cb) refers to s8_demo.o(.data) for sg_system_suspend
    s8_demo.o(i.ap_rstn_pull_high_cb) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    s8_demo.o(i.ap_rstn_pull_high_cb) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.ap_rstn_pull_high_cb) refers to s8_demo.o(.data) for sg_system_resume
    s8_demo.o(i.ap_set_framerate) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode) for hal_dsi_tx_ctrl_set_tear_mode
    s8_demo.o(i.ap_set_framerate) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.ap_set_framerate) refers to s8_demo.o(.data) for FrameRateBackUp
    s8_demo.o(i.ap_update_pps_9E) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) for hal_dsi_rx_ctrl_pre_init_pps
    s8_demo.o(i.ap_update_pps_9E) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) for hal_dsi_rx_ctrl_toggle_resolution
    s8_demo.o(i.ap_update_pps_9E) refers to s8_demo.o(.data) for g_rx_ctrl_handle
    s8_demo.o(i.app_display_init) refers to s8_demo.o(i.app_mipi_rx_init) for app_mipi_rx_init
    s8_demo.o(i.app_display_init) refers to hal_pwr.o(i.hal_pwr_get_vcc_power_ready) for hal_pwr_get_vcc_power_ready
    s8_demo.o(i.app_display_init) refers to s8_demo.o(i.app_gpio_init) for app_gpio_init
    s8_demo.o(i.app_display_init) refers to hal_swire.o(i.hal_swire_init) for hal_swire_init
    s8_demo.o(i.app_display_init) refers to hal_swire.o(i.hal_swire_set_timer) for hal_swire_set_timer
    s8_demo.o(i.app_display_init) refers to s8_demo.o(i.app_mipi_tx_init) for app_mipi_tx_init
    s8_demo.o(i.app_display_init) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.app_gpio_init) refers to memcpya.o(.text) for __aeabi_memcpy4
    s8_demo.o(i.app_gpio_init) refers to hal_gpio.o(i.hal_gpio_config_pad) for hal_gpio_config_pad
    s8_demo.o(i.app_gpio_init) refers to s8_demo.o(.constdata) for .constdata
    s8_demo.o(i.app_init_panel) refers to s8_demo.o(i.app_tx_panel_reset) for app_tx_panel_reset
    s8_demo.o(i.app_init_panel) refers to s8_demo.o(i.send_panel_init_code) for send_panel_init_code
    s8_demo.o(i.app_init_panel) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    s8_demo.o(i.app_init_panel) refers to tau_delay.o(i.delayMs) for delayMs
    s8_demo.o(i.app_init_panel) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    s8_demo.o(i.app_init_panel) refers to s8_demo.o(i.soft_swire_init) for soft_swire_init
    s8_demo.o(i.app_init_panel) refers to hal_swire.o(i.hal_swire_enable) for hal_swire_enable
    s8_demo.o(i.app_init_panel) refers to hal_swire.o(i.hal_swire_set_pulse) for hal_swire_set_pulse
    s8_demo.o(i.app_init_panel) refers to s8_demo.o(.constdata) for panel_init_code
    s8_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) for hal_dsi_rx_ctrl_create_handle
    s8_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) for hal_dsi_rx_ctrl_pre_init_pps
    s8_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    s8_demo.o(i.app_mipi_rx_init) refers to s8_demo.o(i.app_set_dcs_hw_ack) for app_set_dcs_hw_ack
    s8_demo.o(i.app_mipi_rx_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    s8_demo.o(i.app_mipi_rx_init) refers to s8_demo.o(.data) for g_rx_ctrl_handle
    s8_demo.o(i.app_mipi_rx_init) refers to s8_demo.o(.constdata) for g_cus_rx_dcs_execute_table
    s8_demo.o(i.app_mipi_rx_init) refers to s8_demo.o(i.pps_update_handle) for pps_update_handle
    s8_demo.o(i.app_mipi_rx_start_cb) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    s8_demo.o(i.app_mipi_rx_start_cb) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    s8_demo.o(i.app_mipi_rx_start_cb) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.app_mipi_rx_start_cb) refers to s8_demo.o(.data) for g_rx_ctrl_handle
    s8_demo.o(i.app_mipi_tx_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) for hal_dsi_tx_ctrl_create_handle
    s8_demo.o(i.app_mipi_tx_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    s8_demo.o(i.app_mipi_tx_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) for hal_dsi_tx_ctrl_set_overwrite_rgb
    s8_demo.o(i.app_mipi_tx_init) refers to s8_demo.o(.data) for g_tx_ctrl_handle
    s8_demo.o(i.app_mipi_tx_start) refers to s8_demo.o(i.app_init_panel) for app_init_panel
    s8_demo.o(i.app_mipi_tx_start) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    s8_demo.o(i.app_mipi_tx_start) refers to tau_delay.o(i.delayMs) for delayMs
    s8_demo.o(i.app_mipi_tx_start) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    s8_demo.o(i.app_mipi_tx_start) refers to hal_swire.o(i.hal_swire_set_pulse) for hal_swire_set_pulse
    s8_demo.o(i.app_mipi_tx_start) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.app_mipi_tx_start) refers to s8_demo.o(.data) for g_tx_ctrl_handle
    s8_demo.o(i.app_set_dcs_hw_ack) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack) for hal_dsi_rx_ctrl_set_auto_ack
    s8_demo.o(i.app_set_dcs_hw_ack) refers to s8_demo.o(.data) for g_rx_ctrl_handle
    s8_demo.o(i.app_system_process) refers to s8_demo.o(i.app_system_suspend) for app_system_suspend
    s8_demo.o(i.app_system_process) refers to s8_demo.o(i.app_system_resume) for app_system_resume
    s8_demo.o(i.app_system_process) refers to s8_demo.o(i.app_mipi_tx_start) for app_mipi_tx_start
    s8_demo.o(i.app_system_process) refers to s8_demo.o(.data) for sg_system_suspend
    s8_demo.o(i.app_system_resume) refers to hal_pwr.o(i.hal_pwr_exit_sleep_mode) for hal_pwr_exit_sleep_mode
    s8_demo.o(i.app_system_resume) refers to s8_demo.o(i.app_display_init) for app_display_init
    s8_demo.o(i.app_system_resume) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.app_system_suspend) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) for hal_dsi_tx_ctrl_stop
    s8_demo.o(i.app_system_suspend) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) for hal_dsi_tx_ctrl_deinit
    s8_demo.o(i.app_system_suspend) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) for hal_dsi_rx_ctrl_stop
    s8_demo.o(i.app_system_suspend) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) for hal_dsi_rx_ctrl_deinit
    s8_demo.o(i.app_system_suspend) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    s8_demo.o(i.app_system_suspend) refers to hal_swire.o(i.hal_swire_deinit) for hal_swire_deinit
    s8_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_set_sleep_mode_power) for hal_pwr_set_sleep_mode_power
    s8_demo.o(i.app_system_suspend) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    s8_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_enter_normal_sleep_mode) for hal_pwr_enter_normal_sleep_mode
    s8_demo.o(i.app_system_suspend) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) for hal_pwr_set_stop_sleep_wakeup_pin
    s8_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) for hal_pwr_enter_stop_sleep_mode
    s8_demo.o(i.app_system_suspend) refers to hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode) for hal_pwr_enter_deep_sleep_mode
    s8_demo.o(i.app_system_suspend) refers to s8_demo.o(.data) for g_tx_ctrl_handle
    s8_demo.o(i.app_system_suspend) refers to s8_demo.o(i.ap_rstn_pull_high_cb) for ap_rstn_pull_high_cb
    s8_demo.o(i.app_tx_panel_reset) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    s8_demo.o(i.app_tx_panel_reset) refers to tau_delay.o(i.delayMs) for delayMs
    s8_demo.o(i.pps_update_handle) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) for hal_dsi_rx_ctrl_toggle_resolution
    s8_demo.o(i.pps_update_handle) refers to s8_demo.o(.data) for g_rx_ctrl_handle
    s8_demo.o(i.s8_demo) refers to hal_pwr.o(i.hal_pwr_set_main_power) for hal_pwr_set_main_power
    s8_demo.o(i.s8_demo) refers to s8_demo.o(i.app_display_init) for app_display_init
    s8_demo.o(i.s8_demo) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    s8_demo.o(i.s8_demo) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) for hal_dsi_rx_ctrl_dcs_async_handler
    s8_demo.o(i.s8_demo) refers to s8_demo.o(i.app_system_process) for app_system_process
    s8_demo.o(i.s8_demo) refers to s8_demo.o(.data) for g_rx_ctrl_handle
    s8_demo.o(i.send_panel_init_code) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) for hal_dsi_tx_ctrl_write_array_cmd
    s8_demo.o(i.send_panel_init_code) refers to tau_delay.o(i.delayUs) for delayUs
    s8_demo.o(i.soft_swire_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    s8_demo.o(i.soft_swire_init) refers to tau_delay.o(i.delayMs) for delayMs
    s8_demo.o(i.soft_swire_init) refers to s8_demo.o(i.soft_swire_start) for soft_swire_start
    s8_demo.o(i.soft_swire_init) refers to hal_timer.o(i.hal_timer_init) for hal_timer_init
    s8_demo.o(i.soft_swire_init) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    s8_demo.o(i.soft_swire_init) refers to s8_demo.o(.data) for s_swire_pwm_counter
    s8_demo.o(i.soft_swire_init) refers to s8_demo.o(i.soft_swire_timer_callback) for soft_swire_timer_callback
    s8_demo.o(i.soft_swire_start) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    s8_demo.o(i.soft_swire_start) refers to tau_delay.o(i.delayUs) for delayUs
    s8_demo.o(i.soft_swire_timer_callback) refers to s8_demo.o(i.soft_swire_start) for soft_swire_start
    s8_demo.o(i.soft_swire_timer_callback) refers to hal_timer.o(i.hal_timer_start) for hal_timer_start
    s8_demo.o(i.soft_swire_timer_callback) refers to hal_timer.o(i.hal_timer_deinit) for hal_timer_deinit
    s8_demo.o(i.soft_swire_timer_callback) refers to hal_timer.o(i.hal_timer_stop) for hal_timer_stop
    s8_demo.o(i.soft_swire_timer_callback) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    s8_demo.o(i.soft_swire_timer_callback) refers to s8_demo.o(.data) for s_swire_pwm_counter
    s8_demo.o(.constdata) refers to s8_demo.o(i.ap_dcs_set_display_on) for ap_dcs_set_display_on
    s8_demo.o(.constdata) refers to s8_demo.o(i.ap_dcs_set_display_off) for ap_dcs_set_display_off
    s8_demo.o(.constdata) refers to s8_demo.o(i.ap_dcs_set_backlight) for ap_dcs_set_backlight
    s8_demo.o(.constdata) refers to s8_demo.o(i.ap_dcs_set_enter_sleep_mode) for ap_dcs_set_enter_sleep_mode
    s8_demo.o(.constdata) refers to s8_demo.o(i.ap_dcs_set_exit_sleep_mode) for ap_dcs_set_exit_sleep_mode
    s8_demo.o(.constdata) refers to s8_demo.o(i.ap_update_pps_9E) for ap_update_pps_9E
    s8_demo.o(.constdata) refers to s8_demo.o(i.ap_set_framerate) for ap_set_framerate
    board.o(i.board_Init) refers to hal_system.o(i.hal_system_init) for hal_system_init
    board.o(i.board_Init) refers to tau_log.o(i.tau_log_init) for tau_log_init
    startup_armcm0.o(RESET) refers to startup_armcm0.o(STACK) for __initial_sp
    startup_armcm0.o(RESET) refers to startup_armcm0.o(.text) for Reset_Handler
    startup_armcm0.o(RESET) refers to drv_common.o(i.HardFault_Handler) for HardFault_Handler
    startup_armcm0.o(RESET) refers to drv_common.o(i.SysTick_Handler) for SysTick_Handler
    startup_armcm0.o(RESET) refers to drv_vidc.o(i.VIDC_IRQn_Handler) for VIDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to hal_internal_vsync.o(i.LCDC_IRQn_Handler) for LCDC_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) for MIPI_RX_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler) for MIPI_TX_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_memc.o(i.MEMC_IRQn_Handler) for MEMC_IRQn_Handler
    startup_armcm0.o(RESET) refers to hal_internal_dcs.o(i.VPRE_IRQn_Handler) for VPRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_dma.o(i.DMA_IRQn_Handler) for DMA_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER0_IRQn_Handler) for TIMER0_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER1_IRQn_Handler) for TIMER1_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER2_IRQn_Handler) for TIMER2_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_timer.o(i.TIMER3_IRQn_Handler) for TIMER3_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_wdg.o(i.WDG_IRQn_Handler) for WDG_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_uart.o(i.UART_IRQn_Handler) for UART_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_i2c.o(i.I2C0_IRQn_Handler) for I2C0_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_i2c.o(i.I2C1_IRQn_Handler) for I2C1_IRQn_Handler
    startup_armcm0.o(RESET) refers to hal_spi_master.o(i.SPIM_IRQn_Handler) for SPIM_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_rxbr.o(i.VPRE1_IRQn_Handler) for VPRE1_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_i2c.o(i.I2C2_IRQn_Handler) for I2C2_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_swire.o(i.SWIRE_IRQn_Handler) for SWIRE_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.AP_NRESET_IRQn_Handler) for AP_NRESET_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT0_IRQn_Handler) for EXTI_INT0_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT1_IRQn_Handler) for EXTI_INT1_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT2_IRQn_Handler) for EXTI_INT2_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT3_IRQn_Handler) for EXTI_INT3_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT4_IRQn_Handler) for EXTI_INT4_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT5_IRQn_Handler) for EXTI_INT5_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT6_IRQn_Handler) for EXTI_INT6_IRQn_Handler
    startup_armcm0.o(RESET) refers to drv_gpio.o(i.EXTI_INT7_IRQn_Handler) for EXTI_INT7_IRQn_Handler
    startup_armcm0.o(.text) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    demo_hal_crc.o(i.demo_crc_array_dma_cal) refers to hal_crc.o(i.hal_crc_dma_init) for hal_crc_dma_init
    demo_hal_crc.o(i.demo_crc_array_dma_cal) refers to hal_crc.o(i.hal_crc_dma_start) for hal_crc_dma_start
    demo_hal_crc.o(i.demo_crc_array_dma_cal) refers to demo_hal_crc.o(.constdata) for .constdata
    demo_hal_crc.o(i.demo_crc_array_dma_cal) refers to demo_hal_crc.o(.data) for sg_crc32_arry
    demo_hal_crc.o(i.demo_crc_array_dma_cal) refers to demo_hal_crc.o(i.demo_crc_dma_callback) for demo_crc_dma_callback
    demo_hal_crc.o(i.demo_crc_dma_callback) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    demo_hal_crc.o(i.demo_hal_crc_case) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    demo_hal_crc.o(i.demo_hal_crc_case) refers to demo_hal_crc.o(i.demo_crc_array_dma_cal) for demo_crc_array_dma_cal
    demo_hal_dsi_rx.o(i.ap_dcs_read) refers to memcpya.o(.text) for __aeabi_memcpy4
    demo_hal_dsi_rx.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd) for hal_dsi_rx_ctrl_ack_long_cmd
    demo_hal_dsi_rx.o(i.ap_dcs_read) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) for hal_dsi_rx_ctrl_get_max_ret_size
    demo_hal_dsi_rx.o(i.ap_dcs_read) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    demo_hal_dsi_rx.o(i.ap_dcs_read) refers to demo_hal_dsi_rx.o(.constdata) for .constdata
    demo_hal_dsi_rx.o(i.ap_dcs_read) refers to demo_hal_dsi_rx.o(.data) for g_rx_ctrl_handle
    demo_hal_dsi_rx.o(i.cus_dsc_execute) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    demo_hal_dsi_rx.o(i.cus_dsc_execute) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) for hal_dsi_rx_ctrl_send_ack_cmd
    demo_hal_dsi_rx.o(i.cus_dsc_execute) refers to demo_hal_dsi_rx.o(.data) for g_rx_ctrl_handle
    demo_hal_dsi_rx.o(i.demo_hal_dsi_rx_case) refers to demo_hal_dsi_rx.o(i.open_mipi_rx) for open_mipi_rx
    demo_hal_dsi_rx.o(i.demo_hal_dsi_rx_case) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    demo_hal_dsi_rx.o(i.demo_hal_dsi_rx_case) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) for hal_dsi_rx_ctrl_dcs_async_handler
    demo_hal_dsi_rx.o(i.demo_hal_dsi_rx_case) refers to demo_hal_dsi_rx.o(.data) for g_rx_ctrl_handle
    demo_hal_dsi_rx.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) for hal_dsi_rx_ctrl_create_handle
    demo_hal_dsi_rx.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    demo_hal_dsi_rx.o(i.open_mipi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    demo_hal_dsi_rx.o(i.open_mipi_rx) refers to demo_hal_dsi_rx.o(.data) for g_rx_ctrl_handle
    demo_hal_dsi_rx.o(i.open_mipi_rx) refers to demo_hal_dsi_rx.o(.constdata) for g_cus_rx_dcs_execute_table
    demo_hal_dsi_rx.o(i.open_mipi_rx) refers to demo_hal_dsi_rx.o(i.ap_dcs_read) for ap_dcs_read
    demo_hal_dsi_rx.o(.constdata) refers to demo_hal_dsi_rx.o(i.cus_dsc_execute) for cus_dsc_execute
    demo_hal_dsi_tx.o(i.demo_dsi_tx_case) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    demo_hal_dsi_tx.o(i.demo_dsi_tx_case) refers to demo_hal_dsi_tx.o(i.demo_open_mipi_rx) for demo_open_mipi_rx
    demo_hal_dsi_tx.o(i.demo_dsi_tx_case) refers to demo_hal_dsi_tx.o(i.demo_open_mipi_tx) for demo_open_mipi_tx
    demo_hal_dsi_tx.o(i.demo_open_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) for hal_dsi_tx_ctrl_create_handle
    demo_hal_dsi_tx.o(i.demo_open_mipi_tx) refers to memcpya.o(.text) for __aeabi_memcpy4
    demo_hal_dsi_tx.o(i.demo_open_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    demo_hal_dsi_tx.o(i.demo_open_mipi_tx) refers to demo_hal_dsi_tx.o(i.demo_panel_init) for demo_panel_init
    demo_hal_dsi_tx.o(i.demo_open_mipi_tx) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) for hal_dsi_tx_ctrl_start
    demo_hal_dsi_tx.o(i.demo_open_mipi_tx) refers to demo_hal_dsi_tx.o(.data) for g_tx_ctrl_handle
    demo_hal_dsi_tx.o(i.demo_panel_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    demo_hal_dsi_tx.o(i.demo_panel_init) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    demo_hal_dsi_tx.o(i.demo_panel_init) refers to tau_delay.o(i.delayMs) for delayMs
    demo_hal_dsi_tx.o(i.demo_panel_init) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    demo_hal_dsi_tx.o(i.demo_panel_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) for hal_dsi_tx_ctrl_write_cmd
    demo_hal_wdg.o(i.demo_wdg_callback) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    demo_hal_wdg.o(i.demo_wdg_callback) refers to hal_wdg.o(i.hal_wdg_stop) for hal_wdg_stop
    demo_hal_wdg.o(i.demo_wdg_callback) refers to demo_hal_wdg.o(.data) for sg_wdg_io_lvl
    demo_hal_wdg.o(i.demo_wdg_case) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    demo_hal_wdg.o(i.demo_wdg_case) refers to demo_hal_wdg.o(i.demo_wdg_case_int_mode) for demo_wdg_case_int_mode
    demo_hal_wdg.o(i.demo_wdg_case_int_mode) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    demo_hal_wdg.o(i.demo_wdg_case_int_mode) refers to hal_wdg.o(i.hal_wdg_init) for hal_wdg_init
    demo_hal_wdg.o(i.demo_wdg_case_int_mode) refers to hal_wdg.o(i.hal_wdg_set_repeat) for hal_wdg_set_repeat
    demo_hal_wdg.o(i.demo_wdg_case_int_mode) refers to hal_wdg.o(i.hal_wdg_register_callback) for hal_wdg_register_callback
    demo_hal_wdg.o(i.demo_wdg_case_int_mode) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    demo_hal_wdg.o(i.demo_wdg_case_int_mode) refers to hal_wdg.o(i.hal_wdg_start) for hal_wdg_start
    demo_hal_wdg.o(i.demo_wdg_case_int_mode) refers to hal_wdg.o(i.hal_wdg_kick_dog) for hal_wdg_kick_dog
    demo_hal_wdg.o(i.demo_wdg_case_int_mode) refers to tau_delay.o(i.delayMs) for delayMs
    demo_hal_wdg.o(i.demo_wdg_case_int_mode) refers to demo_hal_wdg.o(i.demo_wdg_callback) for demo_wdg_callback
    demo_hal_wdg.o(i.demo_wdg_case_int_mode) refers to demo_hal_wdg.o(.data) for sg_wdg_io_lvl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd) refers to drv_rxbr.o(i.drv_rxbr_set_ack_pkt_md) for drv_rxbr_set_ack_pkt_md
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_lpdt_fifo_status) for drv_dsi_rx_get_lpdt_fifo_status
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) for dcs_packet_get_fifo_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) refers to dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) for dcs_packet_free_fifo_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) for hal_internal_vsync_get_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_reset_modules) for drv_crgu_reset_modules
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_rxbr.o(i.drv_rxbr_swpxl_clr) for drv_rxbr_swpxl_clr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_rxbr.o(i.drv_rxbr_set_cmd_filter) for drv_rxbr_set_cmd_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_disable) for drv_dsc_dec_disable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_vidc.o(i.drv_vidc_set_src_parameter) for drv_vidc_set_src_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_vidc.o(i.drv_vidc_set_pu_ctrl) for drv_vidc_set_pu_ctrl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to drv_rxbr.o(i.drv_rxbr_set_swpxl_data) for drv_rxbr_set_swpxl_data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg) for drv_dsi_rx_set_ddi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) for hal_dsi_rx_ctrl_set_rx_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg) for drv_dsi_rx_set_ipi_pg_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.constdata) for .constdata
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_force_video_crtl) refers to drv_dsi_rx.o(i.drv_dsi_rx_force_video_crtl) for drv_dsi_rx_force_video_crtl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size) for drv_dsi_rx_get_max_ret_size
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) for hal_dsi_rx_ctrl_init_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_rx) for hal_internal_vsync_init_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) for hal_dsi_rx_ctrl_init_dsi_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) for hal_dsi_rx_ctrl_init_rxbr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_dsc_dec.o(i.drv_dsc_dec_set_irqen) for drv_dsc_dec_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) for hal_dsi_rx_ctrl_init_vidc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) for hal_dsi_rx_ctrl_init_memc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to drv_se.o(i.drv_se_start_rx) for drv_se_start_rx
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_pwr.o(i.drv_pwr_set_pll_clk) for drv_pwr_set_pll_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_clk) for drv_crgu_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_dsc_clk) for drv_crgu_set_dsc_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_vidc_clk) for drv_crgu_set_vidc_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_set_fb_clk) for drv_crgu_set_fb_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg) for drv_dsi_rx_set_ctrl_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) for drv_dsi_rx_set_up_phy
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap) for drv_dsi_rx_set_lane_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_crc_en) for drv_dsi_rx_set_ddi_crc_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_ycbcr_frmt) for drv_dsi_rx_set_ipi_ycbcr_frmt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_tear_resp_en) for drv_dsi_rx_set_tear_resp_en
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_inten) for drv_dsi_rx_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc) for drv_dsi_rx_set_check_crc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt) for drv_dsi_rx_set_resp_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) for drv_dsi_rx_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_mode) for drv_memc_set_ltpo_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_fs_en_conditions) for drv_memc_set_fs_en_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_lcdc_st_conditions) for drv_memc_set_lcdc_st_conditions
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_vidc_sync_cnt) for drv_memc_set_vidc_sync_cnt
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_waveform) for drv_memc_set_tear_waveform
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_double_buffer) for drv_memc_set_double_buffer
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_circ_mode_enable) for drv_memc_set_circ_mode_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_active_height) for drv_memc_set_active_height
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_set_ltpo_pu_thres) for drv_memc_set_ltpo_pu_thres
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to drv_memc.o(i.drv_memc_enable_irq) for drv_memc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_color_format) for drv_rxbr_set_color_format
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th) for drv_rxbr_set_ltpo_drop_th
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_cfg) for drv_rxbr_set_usr_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_col) for drv_rxbr_set_usr_col
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_set_usr_row) for drv_rxbr_set_usr_row
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg) for drv_rxbr_hline_rcv_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to drv_rxbr.o(i.drv_rxbr_enable_irq) for drv_rxbr_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) for hal_intl_dcs_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_src_parameter) for drv_vidc_set_src_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pentile_swap) for drv_vidc_set_pentile_swap
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_dst_parameter) for drv_vidc_set_dst_parameter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_circ_mode_enable) for drv_vidc_set_circ_mode_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_init_module_enable) for drv_vidc_init_module_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_dither_config) for drv_vidc_set_dither_config
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_vintp_config) for drv_vidc_set_vintp_config
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_rotation) for drv_vidc_set_rotation
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_step) for drv_vidc_set_scld_step
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef0) for drv_vidc_set_scld_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_hcoef1) for drv_vidc_set_scld_hcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef0) for drv_vidc_set_scld_vcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_scld_vcoef1) for drv_vidc_set_scld_vcoef1
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_honly_hinitr) for drv_vidc_set_honly_hinitr
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_honly_hinitb) for drv_vidc_set_honly_hinitb
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_honly_hcoef0) for drv_vidc_set_honly_hcoef0
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_mirror) for drv_vidc_set_mirror
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_pu_ctrl) for drv_vidc_set_pu_ctrl
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to drv_vidc.o(i.drv_vidc_enable_irq) for drv_vidc_enable_irq
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc) refers to hal_dsi_rx_ctrl.o(.constdata) for .constdata
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to hal_internal_vsync.o(i.hal_internal_sync_register_rx_callback) for hal_internal_sync_register_rx_callback
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to drv_vidc.o(i.drv_vidc_set_irq_line) for drv_vidc_set_irq_line
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_write_cmd_entry) refers to hal_internal_dcs.o(i.hal_intl_dcs_register_write_cmd_entry) for hal_intl_dcs_register_write_cmd_entry
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header) for drv_rxbr_set_ack_pkt_header
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack) refers to drv_rxbr.o(i.drv_rxbr_set_cmd_response) for drv_rxbr_set_cmd_response
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack) refers to hal_dsi_rx_ctrl.o(.conststring) for .conststring
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) for hal_intl_dcs_set_auto_hw_filter
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_check_crc) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc) for drv_dsi_rx_set_check_crc
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_check_crc) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) for drv_dsi_rx_calc_ipi_tx_delay
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg) for drv_dsi_rx_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_log_level) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_drv_log_level) for drv_dsi_rx_set_drv_log_level
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to drv_rxbr.o(i.drv_rxbr_sw_reset) for drv_rxbr_sw_reset
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) for hal_dsi_rx_ctrl_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) for hal_intl_svs_update_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg) for drv_dsi_rx_set_ddi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg) for hal_dsi_rx_ctrl_set_ipi_cfg
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk) refers to hal_dsi_rx_ctrl.o(.data) for .data
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_set_rxbr_clk) for drv_crgu_set_rxbr_clk
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to drv_dsi_rx.o(i.drv_dsi_rx_power_up) for drv_dsi_rx_power_up
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to drv_dsi_rx.o(i.drv_dsi_rx_shut_down) for drv_dsi_rx_shut_down
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) for hal_internal_vsync_set_rx_state
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate) refers to hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) for hal_internal_vsync_toggle_input_frame_rate
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) for hal_internal_sync_input_resolution_change
    hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution) refers to hal_dsi_rx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to fadd.o(.text) for __aeabi_fadd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) for hal_dsi_tx_ctrl_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg) for drv_dsi_tx_phy_time_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) for drv_dsi_tx_phy_test_setup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready) for drv_dsi_tx_phy_status_ready
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to drv_crgu.o(i.drv_crgu_reset_modules) for drv_crgu_reset_modules
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to drv_crgu.o(i.drv_crgu_reset_modules) for drv_crgu_reset_modules
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb) for hal_internal_sync_register_lcdc_cb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) for hal_internal_sync_set_fb_setting_manual
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) for hal_lcdc_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to drv_memc.o(i.drv_memc_set_data_mode) for drv_memc_set_data_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_frame) refers to drv_lcdc.o(i.drv_lcdc_fixed_frame_output) for drv_lcdc_fixed_frame_output
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_get_tear_mode) for drv_memc_get_tear_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) refers to drv_memc.o(i.drv_memc_gen_a_tear_signal) for drv_memc_gen_a_tear_signal
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_init_tx) for hal_internal_vsync_init_tx
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb) for hal_internal_sync_register_lcdc_cb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) for hal_dsi_tx_ctrl_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) for hal_dsi_tx_init_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) for hal_dsi_tx_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) for hal_lcdc_init_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) for hal_lcdc_init_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready) for drv_dsi_tx_phy_status_ready
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) for hal_nonshadow_func_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) refers to hal_dsi_tx_ctrl.o(i.hal_vsync_func_update) for hal_vsync_func_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_overwrite_enable) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_overwrite_enable) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_partial_disp_enable) refers to drv_lcdc.o(i.drv_lcdc_part_display_config) for drv_lcdc_part_display_config
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_partial_disp_enable) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload) for drv_dsi_tx_command_get_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) for hal_nonshadow_func_req_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_sync_line) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) for hal_internal_vsync_set_sync_line
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_sync_line) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) for hal_nonshadow_func_req_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to memcpya.o(.text) for __aeabi_memcpy
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) for hal_nonshadow_func_req_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc) refers to hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) for hal_nonshadow_func_req_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb) refers to drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb) for drv_lcdc_config_overwrite_rgb
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) for hal_internal_vsync_set_tear_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_vpg) for drv_dsi_tx_set_vpg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick) for hal_dsi_tx_ctrl_draw_flick
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp) for drv_dsi_tx_phy_clock_lane_auto_lp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_cfg_int_frame) for drv_lcdc_cfg_int_frame
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_dsi_tx.o(i.drv_dsi_tx_powerup) for drv_dsi_tx_powerup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to drv_lcdc.o(i.drv_lcdc_enable_shadow_reg) for drv_lcdc_enable_shadow_reg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_start) for hal_lcdc_start
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_lcdc.o(i.drv_lcdc_stop_display) for drv_lcdc_stop_display
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to drv_dsi_tx.o(i.drv_dsi_tx_shutdown) for drv_dsi_tx_shutdown
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd) for hal_dsi_tx_ctrl_read_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) for hal_dsi_tx_send_cmd
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg) for drv_dsi_tx_video_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack) for drv_dsi_tx_set_bta_ack
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time) for drv_dsi_tx_dpi_lpcmd_time
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg) for drv_dsi_tx_command_mode_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_mode) for drv_dsi_tx_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode) for drv_dsi_tx_phy_lane_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode) for drv_dsi_tx_dpi_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity) for drv_dsi_tx_dpi_polarity
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_response_mode) for drv_dsi_tx_response_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_eotp) for drv_dsi_tx_config_eotp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div) for drv_dsi_tx_set_esc_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div) for drv_dsi_tx_set_time_out_div
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to memseta.o(.text) for __aeabi_memclr4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg) for drv_dsi_tx_timeout_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp) for drv_dsi_tx_phy_clock_lane_auto_lp
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_config_int) for drv_dsi_tx_config_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_int) for drv_dsi_tx_set_int
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to drv_crgu.o(i.drv_crgu_set_dpi_clk) for drv_crgu_set_dpi_clk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) refers to hal_dsi_tx_ctrl.o(.constdata) for .constdata
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg) for drv_dsi_tx_phy_time_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) for drv_dsi_tx_phy_test_setup
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update) for hal_dsi_tx_timing_info_update
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing) for hal_dsi_tx_cmd_mode_cal_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size) for drv_dsi_tx_edpi_cmd_size
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg) for hal_dsi_tx_init_phy_cfg
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing) for hal_dsi_tx_init_dpi_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) for hal_dsi_tx_vid_mode_cal_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing) for hal_dsi_tx_init_vid_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk) for drv_dsi_tx_set_video_chunk
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing) refers to drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing) for drv_dsi_tx_set_video_timing
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status) for drv_dsi_tx_get_cmd_status
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_header) for drv_dsi_tx_command_header
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update) refers to d2f.o(.text) for __aeabi_d2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to fmul.o(.text) for __aeabi_fmul
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to idiv.o(.text) for __aeabi_idivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_internal_svs.o(i.hal_intl_svs_init_tx) for hal_intl_svs_init_tx
    hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing) refers to hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) for hal_tx_frame_rate_adjust
    hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) refers to drv_lcdc.o(i.drv_lcdc_endianness_config) for drv_lcdc_endianness_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) refers to drv_lcdc.o(i.drv_lcdc_crop_hact) for drv_lcdc_crop_hact
    hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) for hal_lcdc_postproc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config) for hal_lcdc_displayproc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) for hal_intl_fb_get_tx_fb_info
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) for hal_lcdc_timinggen_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to drv_lcdc.o(i.drv_lcdc_config_int) for drv_lcdc_config_int
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg) refers to drv_lcdc.o(i.drv_lcdc_set_int) for drv_lcdc_set_int
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fscalb.o(.text) for __ARM_scalbnf
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to f2d.o(.text) for __aeabi_f2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to ceil.o(i.ceil) for ceil
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk) refers to drv_crgu.o(i.drv_crgu_set_lcdc_clk) for drv_crgu_set_lcdc_clk
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) for hal_intl_fb_get_tx_fb_info
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) for hal_lcdc_upscaler_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_fldc_config) for drv_lcdc_fldc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_bcsa_config) for drv_lcdc_bcsa_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_fc_config) for drv_lcdc_fc_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_edge_dect_config) for drv_lcdc_edge_dect_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_edge_enh_config) for drv_lcdc_edge_enh_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_vintp_mode_config) for drv_lcdc_vintp_mode_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to drv_lcdc.o(i.drv_lcdc_dith_config) for drv_lcdc_dith_config
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for .ARM.__at_0x1102C
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to drv_lcdc.o(i.drv_lcdc_vid_hw_start) for drv_lcdc_vid_hw_start
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_dsi_tx_ctrl.o(i.hal_lcdc_start) refers to drv_lcdc.o(i.drv_lcdc_cmd_start) for drv_lcdc_cmd_start
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to drv_lcdc.o(i.drv_lcdc_ctrl_flow) for drv_lcdc_ctrl_flow
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to drv_lcdc.o(i.drv_lcdc_config_src_parameter) for drv_lcdc_config_src_parameter
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) for hal_intl_fb_get_memc_flow_mode
    hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config) refers to drv_lcdc.o(i.drv_lcdc_set_prefetch) for drv_lcdc_set_prefetch
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to dadd.o(.text) for __aeabi_dadd
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for sg_pq_para
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_bcsa_config) for drv_lcdc_bcsa_config
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_fc_config) for drv_lcdc_fc_config
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_edge_dect_config) for drv_lcdc_edge_dect_config
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_edge_enh_config) for drv_lcdc_edge_enh_config
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update) refers to hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C) for sg_pq_para
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to cfcmple.o(.text) for __aeabi_cfcmple
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init) for hal_dsi_tx_ctrl_init
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) for hal_internal_vsync_set_tx_state
    hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust) refers to hal_dsi_tx_ctrl.o(.bss) for .bss
    hal_dsi_tx_ctrl.o(i.hal_vsync_func_update) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_dsi_tx_ctrl.o(i.hal_vsync_func_update) refers to hal_dsi_tx_ctrl.o(.data) for .data
    hal_gpio.o(i.hal_gpio_config_pad) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_config_pad) refers to hal_gpio.o(i.hal_gpio_init_input) for hal_gpio_init_input
    hal_gpio.o(i.hal_gpio_config_pad) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    hal_gpio.o(i.hal_gpio_ctrl_eint) refers to drv_gpio.o(i.drv_gpio_set_int) for drv_gpio_set_int
    hal_gpio.o(i.hal_gpio_get_input_data) refers to drv_gpio.o(i.drv_gpio_get_input_data) for drv_gpio_get_input_data
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_get_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_eint) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group) for drv_sys_cfg_sel_gpio_group
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig) for drv_sys_cfg_sel_int_trig
    hal_gpio.o(i.hal_gpio_init_eint) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_init_input) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_input) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_init_output) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_init_output) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_reg_eint_cb) refers to drv_gpio.o(i.drv_gpio_register_callback) for drv_gpio_register_callback
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_gpio.o(i.drv_gpio_register_ap_reset_callback) for drv_gpio_register_ap_reset_callback
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig) for drv_sys_cfg_sel_ap_rst_trig
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_gpio.o(i.hal_gpio_set_ap_reset_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_driving_strength) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_high_impedance) refers to drv_gpio.o(i.drv_gpio_set_ioe) for drv_gpio_set_ioe
    hal_gpio.o(i.hal_gpio_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_gpio.o(i.hal_gpio_set_high_impedance) refers to hal_gpio.o(i.hal_gpio_set_pull_state) for hal_gpio_set_pull_state
    hal_gpio.o(i.hal_gpio_set_mode) refers to drv_gpio.o(i.drv_gpio_set_mode) for drv_gpio_set_mode
    hal_gpio.o(i.hal_gpio_set_mode) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_output_data) refers to hal_gpio.o(i.drv_gpio_set_output_data) for drv_gpio_set_output_data
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_pull_state) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_schmitt_trigger) refers to hal_gpio.o(.constdata) for .constdata
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to drv_gpio.o(i.drv_gpio_get_attribute) for drv_gpio_get_attribute
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to drv_gpio.o(i.drv_gpio_set_attribute) for drv_gpio_set_attribute
    hal_gpio.o(i.hal_gpio_set_slew_rate) refers to hal_gpio.o(.constdata) for .constdata
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_i2c.o(i.drv_i2c_get_intr_status) for drv_i2c_get_intr_status
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_i2c.o(i.drv_i2c_get_rx_count) for drv_i2c_get_rx_count
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_i2c.o(i.drv_i2c_flush) for drv_i2c_flush
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_i2c.o(i.drv_i2c_clear_intr_status) for drv_i2c_clear_intr_status
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_dma.o(i.drv_dma_get_remaining_trans_num) for drv_dma_get_remaining_trans_num
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_dma.o(i.drv_dma_set_mem_trans_offset) for drv_dma_set_mem_trans_offset
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_dma.o(i.drv_dma_enable) for drv_dma_enable
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_i2c.o(i.drv_i2c_get_fifo_status) for drv_i2c_get_fifo_status
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_i2c.o(i.drv_i2c_get_tx_abrtsource) for drv_i2c_get_tx_abrtsource
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to drv_i2c.o(i.drv_i2c_write_data) for drv_i2c_write_data
    hal_i2c_slave.o(i.hal_i2cs_callback) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_deinit) refers to drv_dma.o(i.drv_dma_deinit) for drv_dma_deinit
    hal_i2c_slave.o(i.hal_i2cs_deinit) refers to drv_i2c.o(i.drv_i2c_clock_enable) for drv_i2c_clock_enable
    hal_i2c_slave.o(i.hal_i2cs_deinit) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_get_rx_cnt) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_get_tx_cnt) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_get_write_complete) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_init) refers to drv_i2c.o(i.drv_i2c_clock_enable) for drv_i2c_clock_enable
    hal_i2c_slave.o(i.hal_i2cs_init) refers to drv_i2c.o(i.drv_i2cs_init) for drv_i2cs_init
    hal_i2c_slave.o(i.hal_i2cs_init) refers to drv_i2c.o(i.drv_i2c_set_callback) for drv_i2c_set_callback
    hal_i2c_slave.o(i.hal_i2cs_init) refers to drv_dma.o(i.drv_dma_apply_handle) for drv_dma_apply_handle
    hal_i2c_slave.o(i.hal_i2cs_init) refers to drv_dma.o(i.drv_dma_set_bitwide) for drv_dma_set_bitwide
    hal_i2c_slave.o(i.hal_i2cs_init) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    hal_i2c_slave.o(i.hal_i2cs_init) refers to hal_i2c_slave.o(i.hal_i2cs_callback) for hal_i2cs_callback
    hal_i2c_slave.o(i.hal_i2cs_init) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_register_callback) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_rx_cnt_clear) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_set_continue_transfer) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_start) refers to drv_i2c.o(i.drv_i2c_enable_intr) for drv_i2c_enable_intr
    hal_i2c_slave.o(i.hal_i2cs_start) refers to drv_i2c.o(i.drv_i2c_enable) for drv_i2c_enable
    hal_i2c_slave.o(i.hal_i2cs_start) refers to drv_i2c.o(i.drv_i2c_enable_dma_req) for drv_i2c_enable_dma_req
    hal_i2c_slave.o(i.hal_i2cs_start) refers to drv_dma.o(i.drv_dma_register_callback) for drv_dma_register_callback
    hal_i2c_slave.o(i.hal_i2cs_start) refers to drv_dma.o(i.drv_dma_enable_int) for drv_dma_enable_int
    hal_i2c_slave.o(i.hal_i2cs_start) refers to drv_dma.o(i.drv_dma_enable) for drv_dma_enable
    hal_i2c_slave.o(i.hal_i2cs_start) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_start) refers to hal_i2c_slave.o(i.hal_i2cs_tx_dma_callback) for hal_i2cs_tx_dma_callback
    hal_i2c_slave.o(i.hal_i2cs_stop) refers to drv_i2c.o(i.drv_i2c_enable) for drv_i2c_enable
    hal_i2c_slave.o(i.hal_i2cs_stop) refers to drv_i2c.o(i.drv_i2c_disable_intr) for drv_i2c_disable_intr
    hal_i2c_slave.o(i.hal_i2cs_stop) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_i2c_slave.o(i.hal_i2cs_stop) refers to drv_i2c.o(i.drv_i2c_disable_dma_req) for drv_i2c_disable_dma_req
    hal_i2c_slave.o(i.hal_i2cs_stop) refers to drv_i2c.o(i.drv_i2c_flush) for drv_i2c_flush
    hal_i2c_slave.o(i.hal_i2cs_stop) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_tx_dma_callback) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) refers to drv_i2c.o(i.drv_i2c_disable_dma_req) for drv_i2c_disable_dma_req
    hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) refers to drv_i2c.o(i.drv_i2c_flush) for drv_i2c_flush
    hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) refers to drv_dma.o(i.drv_dma_set_mem_trans_info) for drv_dma_set_mem_trans_info
    hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) refers to drv_dma.o(i.drv_dma_enable) for drv_dma_enable
    hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) refers to drv_i2c.o(i.drv_i2c_enable_dma_req) for drv_i2c_enable_dma_req
    hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer) refers to hal_i2c_slave.o(.data) for .data
    hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer) refers to drv_i2c.o(i.drv_i2c_flush) for drv_i2c_flush
    hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer) refers to drv_dma.o(i.drv_dma_set_mem_trans_info) for drv_dma_set_mem_trans_info
    hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer) refers to drv_dma.o(i.drv_dma_set_circle_mode) for drv_dma_set_circle_mode
    hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer) refers to hal_i2c_slave.o(.data) for .data
    hal_spi_master.o(i.SPIM_IRQn_Handler) refers to drv_spi_master.o(i.drv_spim_disable_int) for drv_spim_disable_int
    hal_spi_master.o(i.SPIM_IRQn_Handler) refers to drv_spi_master.o(i.drv_spim_set_inten) for drv_spim_set_inten
    hal_spi_master.o(i.SPIM_IRQn_Handler) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    hal_spi_master.o(i.SPIM_IRQn_Handler) refers to drv_spi_master.o(i.drv_spim_clear_int_status) for drv_spim_clear_int_status
    hal_spi_master.o(i.SPIM_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_spi_master.o(i.SPIM_IRQn_Handler) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spim_deinit) refers to drv_per_common.o(i.drv_per_set_clock) for drv_per_set_clock
    hal_spi_master.o(i.hal_spim_deinit) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spim_get_transfer_complete) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spim_init) refers to drv_per_common.o(i.drv_per_set_clock) for drv_per_set_clock
    hal_spi_master.o(i.hal_spim_init) refers to hal_gpio.o(i.hal_gpio_init_output) for hal_gpio_init_output
    hal_spi_master.o(i.hal_spim_init) refers to drv_spi_master.o(i.drv_spim_init) for drv_spim_init
    hal_spi_master.o(i.hal_spim_read) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    hal_spi_master.o(i.hal_spim_read) refers to drv_spi_master.o(i.drv_spim_read) for drv_spim_read
    hal_spi_master.o(i.hal_spim_read) refers to hal_spi_master.o(.data) for .data
    hal_spi_master.o(i.hal_spim_write) refers to hal_gpio.o(i.hal_gpio_set_output_data) for hal_gpio_set_output_data
    hal_spi_master.o(i.hal_spim_write) refers to drv_spi_master.o(i.drv_spim_write) for drv_spim_write
    hal_spi_master.o(i.hal_spim_write) refers to hal_spi_master.o(.data) for .data
    hal_swire.o(i.hal_swire_deinit) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    hal_swire.o(i.hal_swire_deinit) refers to drv_swire.o(i.drv_swire_enable) for drv_swire_enable
    hal_swire.o(i.hal_swire_deinit) refers to drv_swire.o(i.drv_swire_register_callback) for drv_swire_register_callback
    hal_swire.o(i.hal_swire_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_swire.o(i.hal_swire_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_swire.o(i.hal_swire_deinit) refers to hal_timer.o(i.hal_timer_deinit) for hal_timer_deinit
    hal_swire.o(i.hal_swire_deinit) refers to hal_swire.o(.data) for .data
    hal_swire.o(i.hal_swire_enable) refers to drv_swire.o(i.drv_swire_set_power_down) for drv_swire_set_power_down
    hal_swire.o(i.hal_swire_enable) refers to drv_swire.o(i.drv_swire_get_pulse_count) for drv_swire_get_pulse_count
    hal_swire.o(i.hal_swire_enable) refers to drv_swire.o(i.drv_swire_set_trig_mode) for drv_swire_set_trig_mode
    hal_swire.o(i.hal_swire_enable) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_swire.o(i.hal_swire_enable) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    hal_swire.o(i.hal_swire_enable) refers to hal_swire.o(.data) for .data
    hal_swire.o(i.hal_swire_init) refers to drv_crgu.o(i.drv_crgu_set_clock_div) for drv_crgu_set_clock_div
    hal_swire.o(i.hal_swire_init) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_swire.o(i.hal_swire_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_swire.o(i.hal_swire_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_swire.o(i.hal_swire_init) refers to drv_swire.o(i.drv_swire_set_bit_time) for drv_swire_set_bit_time
    hal_swire.o(i.hal_swire_init) refers to drv_swire.o(i.drv_swire_set_power_down) for drv_swire_set_power_down
    hal_swire.o(i.hal_swire_init) refers to drv_swire.o(i.drv_swire_enable) for drv_swire_enable
    hal_swire.o(i.hal_swire_init) refers to drv_common.o(.data) for g_system_clock
    hal_swire.o(i.hal_swire_register_callback) refers to drv_swire.o(i.drv_swire_register_callback) for drv_swire_register_callback
    hal_swire.o(i.hal_swire_register_callback) refers to drv_swire.o(i.drv_swire_set_int) for drv_swire_set_int
    hal_swire.o(i.hal_swire_set_pulse) refers to drv_swire.o(i.drv_swire_set_trig_mode) for drv_swire_set_trig_mode
    hal_swire.o(i.hal_swire_set_pulse) refers to drv_swire.o(i.drv_swire_set_pulse_count) for drv_swire_set_pulse_count
    hal_swire.o(i.hal_swire_set_pulse) refers to hal_swire.o(.data) for .data
    hal_swire.o(i.hal_swire_set_timer) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_swire_timer) for drv_sys_cfg_sel_swire_timer
    hal_swire.o(i.hal_swire_set_timer) refers to hal_timer.o(i.hal_timer_init) for hal_timer_init
    hal_swire.o(i.hal_swire_set_timer) refers to hal_timer.o(i.hal_timer_set_repeat) for hal_timer_set_repeat
    hal_swire.o(i.hal_swire_set_timer) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_swire.o(i.hal_swire_set_timer) refers to drv_swire.o(i.drv_swire_set_trig_mode) for drv_swire_set_trig_mode
    hal_swire.o(i.hal_swire_set_timer) refers to hal_swire.o(.data) for .data
    hal_swire.o(i.hal_swire_set_waveform) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_swire.o(i.hal_swire_set_waveform) refers to drv_swire.o(i.drv_swire_set_bit_time) for drv_swire_set_bit_time
    hal_swire.o(i.hal_swire_set_waveform) refers to drv_common.o(.data) for g_system_clock
    hal_system.o(i.hal_system_disable_systick) refers to drv_common.o(i.drv_common_disable_systick) for drv_common_disable_systick
    hal_system.o(i.hal_system_enable_systick) refers to drv_common.o(i.drv_common_enable_systick) for drv_common_enable_systick
    hal_system.o(i.hal_system_get_tick) refers to drv_common.o(i.drv_common_get_tick) for drv_common_get_tick
    hal_system.o(i.hal_system_idle_mode) refers to drv_common.o(i.drv_common_idle_mode) for drv_common_idle_mode
    hal_system.o(i.hal_system_init) refers to drv_pwr.o(i.drv_pwr_set_pll_clk) for drv_pwr_set_pll_clk
    hal_system.o(i.hal_system_init) refers to hal_system.o(i.hal_system_updata_sysclk) for hal_system_updata_sysclk
    hal_system.o(i.hal_system_init) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_system.o(i.hal_system_init) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int) for drv_sys_cfg_clear_all_int
    hal_system.o(i.hal_system_init) refers to drv_common.o(i.drv_common_system_init) for drv_common_system_init
    hal_system.o(i.hal_system_init) refers to hal_gpio.o(i.hal_gpio_set_mode) for hal_gpio_set_mode
    hal_system.o(i.hal_system_register_systick_cb) refers to drv_common.o(i.drv_common_systick_register_cb) for drv_common_systick_register_cb
    hal_system.o(i.hal_system_reset_chip) refers to drv_crgu.o(i.drv_crgu_reset_chip) for drv_crgu_reset_chip
    hal_system.o(i.hal_system_updata_sysclk) refers to drv_crgu.o(i.drv_crgu_set_ahb_clk) for drv_crgu_set_ahb_clk
    hal_system.o(i.hal_system_updata_sysclk) refers to drv_common.o(.data) for g_system_clock
    hal_system.o(i.hal_system_updata_sysclk) refers to drv_common.o(.data) for g_system_delay_step
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_set_repeat) for drv_timer_set_repeat
    hal_timer.o(i.hal_timer_deinit) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_timer.o(i.hal_timer_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_timer.o(i.hal_timer_get_status) refers to drv_timer.o(i.drv_timer_get_status) for drv_timer_get_status
    hal_timer.o(i.hal_timer_init) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_timer.o(i.hal_timer_init) refers to drv_timer.o(i.drv_timer_set_prescaler) for drv_timer_set_prescaler
    hal_timer.o(i.hal_timer_set_repeat) refers to drv_timer.o(i.drv_timer_set_repeat) for drv_timer_set_repeat
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_start) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_start_ex) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_enable) for drv_timer_enable
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_register_callback) for drv_timer_register_callback
    hal_timer.o(i.hal_timer_stop) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    hal_wdg.o(i.hal_wdg_deinit) refers to drv_wdg.o(i.drv_wdg_set_int) for drv_wdg_set_int
    hal_wdg.o(i.hal_wdg_deinit) refers to drv_wdg.o(i.drv_wdg_set_repeat) for drv_wdg_set_repeat
    hal_wdg.o(i.hal_wdg_deinit) refers to drv_wdg.o(i.drv_wdg_enable) for drv_wdg_enable
    hal_wdg.o(i.hal_wdg_deinit) refers to drv_wdg.o(i.drv_wdg_register_callback) for drv_wdg_register_callback
    hal_wdg.o(i.hal_wdg_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_wdg.o(i.hal_wdg_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_wdg.o(i.hal_wdg_init) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_wdg.o(i.hal_wdg_kick_dog) refers to drv_wdg.o(i.drv_wdg_set_int) for drv_wdg_set_int
    hal_wdg.o(i.hal_wdg_kick_dog) refers to drv_wdg.o(i.drv_wdg_clear_counter) for drv_wdg_clear_counter
    hal_wdg.o(i.hal_wdg_register_callback) refers to drv_wdg.o(i.drv_wdg_register_callback) for drv_wdg_register_callback
    hal_wdg.o(i.hal_wdg_set_repeat) refers to drv_wdg.o(i.drv_wdg_set_repeat) for drv_wdg_set_repeat
    hal_wdg.o(i.hal_wdg_start) refers to drv_wdg.o(i.drv_wdg_enable) for drv_wdg_enable
    hal_wdg.o(i.hal_wdg_start) refers to drv_wdg.o(i.drv_wdg_sel_mode) for drv_wdg_sel_mode
    hal_wdg.o(i.hal_wdg_start) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_wdg.o(i.hal_wdg_start) refers to drv_wdg.o(i.drv_wdg_load_match) for drv_wdg_load_match
    hal_wdg.o(i.hal_wdg_start) refers to drv_wdg.o(i.drv_wdg_set_int) for drv_wdg_set_int
    hal_wdg.o(i.hal_wdg_stop) refers to drv_wdg.o(i.drv_wdg_set_int) for drv_wdg_set_int
    hal_wdg.o(i.hal_wdg_stop) refers to drv_wdg.o(i.drv_wdg_clear_counter) for drv_wdg_clear_counter
    hal_wdg.o(i.hal_wdg_stop) refers to drv_wdg.o(i.drv_wdg_enable) for drv_wdg_enable
    hal_crc.o(i.hal_crc_cal) refers to drv_crc.o(i.drv_crc_get_tcrc_register) for drv_crc_get_tcrc_register
    hal_crc.o(i.hal_crc_cal) refers to drv_crc.o(i.drv_crc_get_idr_counter) for drv_crc_get_idr_counter
    hal_crc.o(i.hal_crc_cal) refers to drv_crc.o(i.drv_crc_write_data_register) for drv_crc_write_data_register
    hal_crc.o(i.hal_crc_cal) refers to drv_crc.o(i.drv_crc_get_data_register) for drv_crc_get_data_register
    hal_crc.o(i.hal_crc_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_crc.o(i.hal_crc_dma_callback) refers to drv_crc.o(i.drv_crc_get_idr_counter) for drv_crc_get_idr_counter
    hal_crc.o(i.hal_crc_dma_callback) refers to drv_crc.o(i.drv_crc_get_data_register) for drv_crc_get_data_register
    hal_crc.o(i.hal_crc_dma_callback) refers to drv_crc.o(i.drv_crc_dma_disable) for drv_crc_dma_disable
    hal_crc.o(i.hal_crc_dma_callback) refers to hal_crc.o(.data) for .data
    hal_crc.o(i.hal_crc_dma_deinit) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_crc.o(i.hal_crc_dma_deinit) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_crc.o(i.hal_crc_dma_deinit) refers to drv_dma.o(i.drv_dma_deinit) for drv_dma_deinit
    hal_crc.o(i.hal_crc_dma_deinit) refers to hal_crc.o(.data) for .data
    hal_crc.o(i.hal_crc_dma_init) refers to hal_crc.o(i.hal_crc_init) for hal_crc_init
    hal_crc.o(i.hal_crc_dma_init) refers to drv_dma.o(i.drv_dma_apply_handle) for drv_dma_apply_handle
    hal_crc.o(i.hal_crc_dma_init) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_crc.o(i.hal_crc_dma_init) refers to drv_crc.o(i.drv_crc_get_tcrc_register) for drv_crc_get_tcrc_register
    hal_crc.o(i.hal_crc_dma_init) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    hal_crc.o(i.hal_crc_dma_init) refers to drv_dma.o(i.drv_dma_enable_int) for drv_dma_enable_int
    hal_crc.o(i.hal_crc_dma_init) refers to drv_dma.o(i.drv_dma_register_callback) for drv_dma_register_callback
    hal_crc.o(i.hal_crc_dma_init) refers to drv_dma.o(i.drv_dma_enable) for drv_dma_enable
    hal_crc.o(i.hal_crc_dma_init) refers to hal_crc.o(.data) for .data
    hal_crc.o(i.hal_crc_dma_init) refers to hal_crc.o(i.hal_crc_dma_callback) for hal_crc_dma_callback
    hal_crc.o(i.hal_crc_dma_start) refers to drv_crc.o(i.drv_crc_dma_enable) for drv_crc_dma_enable
    hal_crc.o(i.hal_crc_init) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_crc.o(i.hal_crc_init) refers to drv_crc.o(i.drv_crc_set_tcrc_register) for drv_crc_set_tcrc_register
    hal_crc.o(i.hal_crc_init) refers to drv_crc.o(i.drv_crc_set_initial_seed_register) for drv_crc_set_initial_seed_register
    hal_crc.o(i.hal_crc_init) refers to drv_crc.o(i.drv_crc_set_polynomial_register) for drv_crc_set_polynomial_register
    hal_crc.o(i.hal_crc_init) refers to drv_crc.o(i.drv_crc_set_rev_in_register) for drv_crc_set_rev_in_register
    hal_crc.o(i.hal_crc_init) refers to drv_crc.o(i.drv_crc_set_rev_out_register) for drv_crc_set_rev_out_register
    hal_crc.o(i.hal_crc_init) refers to drv_crc.o(i.drv_crc_set_fxor_register) for drv_crc_set_fxor_register
    hal_crc.o(i.hal_crc_init) refers to drv_crc.o(i.drv_crc_reset) for drv_crc_reset
    hal_crc.o(i.hal_crc_reset) refers to drv_crc.o(i.drv_crc_reset) for drv_crc_reset
    hal_pwr.o(i.hal_pwr_elvcc_close) refers to drv_pwr.o(i.drv_pwr_pwmled_electric_current) for drv_pwr_pwmled_electric_current
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_pwmled_electric_current) for drv_pwr_pwmled_electric_current
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_hv_ldo_mode_sel) for drv_pwr_hv_ldo_mode_sel
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_hv_ldo_mode_clock_sel) for drv_pwr_hv_ldo_mode_clock_sel
    hal_pwr.o(i.hal_pwr_elvcc_ldo_en) refers to drv_pwr.o(i.drv_pwr_pwmled_driver_current_Big_step) for drv_pwr_pwmled_driver_current_Big_step
    hal_pwr.o(i.hal_pwr_elvcc_vol_set) refers to drv_pwr.o(i.drv_pwr_hv_ldo_voltage_set) for drv_pwr_hv_ldo_voltage_set
    hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode) refers to drv_pwr.o(i.drv_pwr_set_wakeup_type) for drv_pwr_set_wakeup_type
    hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode) for drv_pwr_enter_deep_sleep_mode
    hal_pwr.o(i.hal_pwr_enter_normal_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_sleep_mode_ex) for drv_pwr_enter_sleep_mode_ex
    hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) refers to drv_pwr.o(i.drv_pwr_enter_stop_sleep_mode) for drv_pwr_enter_stop_sleep_mode
    hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode) refers to hal_pwr.o(.data) for .data
    hal_pwr.o(i.hal_pwr_exit_sleep_mode) refers to drv_pwr.o(i.drv_pwr_exit_sleep_mode) for drv_pwr_exit_sleep_mode
    hal_pwr.o(i.hal_pwr_get_reset_flag) refers to drv_crgu.o(i.drv_crgu_get_all_reset_flag) for drv_crgu_get_all_reset_flag
    hal_pwr.o(i.hal_pwr_get_reset_flag) refers to drv_pwr.o(i.drv_pwr_get_wakeflag) for drv_pwr_get_wakeflag
    hal_pwr.o(i.hal_pwr_get_reset_flag) refers to drv_crgu.o(i.drv_crgu_clear_all_reset_flags) for drv_crgu_clear_all_reset_flags
    hal_pwr.o(i.hal_pwr_get_vcc_power_ready) refers to drv_pwr.o(i.drv_pwr_get_power_ready_st) for drv_pwr_get_power_ready_st
    hal_pwr.o(i.hal_pwr_ldo13s_en) refers to drv_pwr.o(i.drv_pwr_ldo13s_en) for drv_pwr_ldo13s_en
    hal_pwr.o(i.hal_pwr_ldo13s_set) refers to drv_pwr.o(i.drv_pwr_ldo13s_set) for drv_pwr_ldo13s_set
    hal_pwr.o(i.hal_pwr_ldo18s_en) refers to drv_pwr.o(i.drv_pwr_ldo18s_en) for drv_pwr_ldo18s_en
    hal_pwr.o(i.hal_pwr_ldo18s_set) refers to drv_pwr.o(i.drv_pwr_ldo18s_set) for drv_pwr_ldo18s_set
    hal_pwr.o(i.hal_pwr_set_main_power) refers to drv_pwr.o(i.drv_pwr_set_digit_power_sel) for drv_pwr_set_digit_power_sel
    hal_pwr.o(i.hal_pwr_set_pvd) refers to drv_pwr.o(i.drv_pwr_set_pvd) for drv_pwr_set_pvd
    hal_pwr.o(i.hal_pwr_set_sleep_mode_power) refers to drv_pwr.o(i.drv_pwr_set_breath_screen_power_sel) for drv_pwr_set_breath_screen_power_sel
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_ctrl_eint) for hal_gpio_ctrl_eint
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_init_eint) for hal_gpio_init_eint
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_reg_eint_cb) for hal_gpio_reg_eint_cb
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_gpio.o(i.hal_gpio_set_ap_reset_int) for hal_gpio_set_ap_reset_int
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_pwr.o(.data) for .data
    hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin) refers to hal_pwr.o(i.stop_sleep_cb) for stop_sleep_cb
    hal_pwr.o(i.hal_pwr_set_vcc_enable) refers to drv_pwr.o(i.drv_pwr_charge_pump_en) for drv_pwr_charge_pump_en
    hal_pwr.o(i.stop_sleep_cb) refers to hal_pwr.o(.data) for .data
    tau_delay.o(i.delayMs) refers to tau_delay.o(i.delayUs) for delayUs
    tau_delay.o(i.delayUs) refers to drv_common.o(.data) for g_system_delay_step
    tau_log.o(i.fgetc) refers to hal_uart.o(i.hal_uart_recv_blocking) for hal_uart_recv_blocking
    tau_log.o(i.fgetc) refers to hal_system.o(i.hal_system_get_debug_state) for hal_system_get_debug_state
    tau_log.o(i.fgetc) refers to hal_system.o(i.hal_system_clear_debug_state) for hal_system_clear_debug_state
    tau_log.o(i.fgetc) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.fputc) refers to tau_log.o(i.tau_log_push_log) for tau_log_push_log
    tau_log.o(i.fputc) refers to hal_uart.o(i.hal_uart_send_blocking) for hal_uart_send_blocking
    tau_log.o(i.fputc) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.tau_log_init) refers to hal_uart.o(i.hal_uart_init) for hal_uart_init
    tau_log.o(i.tau_log_init) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.tau_log_printf) refers to memseta.o(.text) for __aeabi_memclr4
    tau_log.o(i.tau_log_printf) refers to strlen.o(.text) for strlen
    tau_log.o(i.tau_log_printf) refers to printfa.o(i.__0vsprintf) for vsprintf
    tau_log.o(i.tau_log_printf) refers to tau_log.o(i.tau_log_push_log) for tau_log_push_log
    tau_log.o(i.tau_log_printf) refers to printfa.o(i.__0printf) for __2printf
    tau_log.o(i.tau_log_printf) refers to tau_log.o(.data) for g_log_port
    tau_log.o(i.tau_log_printf) refers to tau_log.o(.bss) for g_log_buf
    tau_log.o(i.tau_log_push_log) refers to memcpya.o(.text) for __aeabi_memcpy
    tau_log.o(i.tau_log_push_log) refers to tau_delay.o(i.delayUs) for delayUs
    tau_log.o(.ARM.__at_0x1101C) refers to tau_log.o(.bss) for g_log_buf
    hal_uart.o(i.hal_uart0_rx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart0_tx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart1_rx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart1_tx_dma_cb) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_deinit) refers to drv_uart.o(i.drv_uart_deinit) for drv_uart_deinit
    hal_uart.o(i.hal_uart_deinit) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_uart.o(i.hal_uart_deinit) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_dma_path_close) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_uart.o(i.hal_uart_dma_path_close) refers to drv_dma.o(i.drv_dma_deinit) for drv_dma_deinit
    hal_uart.o(i.hal_uart_dma_path_close) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_apply_handle) for drv_dma_apply_handle
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_set_burst) for drv_dma_set_burst
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_register_callback) for drv_dma_register_callback
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_enable_int) for drv_dma_enable_int
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_set_mem_trans_info) for drv_dma_set_mem_trans_info
    hal_uart.o(i.hal_uart_dma_recv) refers to drv_dma.o(i.drv_dma_enable) for drv_dma_enable
    hal_uart.o(i.hal_uart_dma_recv) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_uart.o(i.hal_uart_dma_recv) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_dma_recv) refers to hal_uart.o(i.hal_uart0_rx_dma_cb) for hal_uart0_rx_dma_cb
    hal_uart.o(i.hal_uart_dma_recv) refers to hal_uart.o(i.hal_uart1_rx_dma_cb) for hal_uart1_rx_dma_cb
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_apply_handle) for drv_dma_apply_handle
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_init) for drv_dma_init
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_set_burst) for drv_dma_set_burst
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_register_callback) for drv_dma_register_callback
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_enable_int) for drv_dma_enable_int
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_disable) for drv_dma_disable
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_set_mem_trans_info) for drv_dma_set_mem_trans_info
    hal_uart.o(i.hal_uart_dma_send) refers to drv_dma.o(i.drv_dma_enable) for drv_dma_enable
    hal_uart.o(i.hal_uart_dma_send) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_uart.o(i.hal_uart_dma_send) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_dma_send) refers to hal_uart.o(i.hal_uart0_tx_dma_cb) for hal_uart0_tx_dma_cb
    hal_uart.o(i.hal_uart_dma_send) refers to hal_uart.o(i.hal_uart1_tx_dma_cb) for hal_uart1_tx_dma_cb
    hal_uart.o(i.hal_uart_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_uart.o(i.hal_uart_init) refers to drv_uart.o(i.drv_uart_init) for drv_uart_init
    hal_uart.o(i.hal_uart_init) refers to drv_uart.o(i.drv_uart_trans_create_handle) for drv_uart_trans_create_handle
    hal_uart.o(i.hal_uart_init) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_init) refers to drv_common.o(.data) for g_system_clock
    hal_uart.o(i.hal_uart_init) refers to hal_uart.o(.data) for .data
    hal_uart.o(i.hal_uart_recv_blocking) refers to drv_uart.o(i.drv_uart_recv_blocking) for drv_uart_recv_blocking
    hal_uart.o(i.hal_uart_recv_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_recv_none_blocking) refers to drv_uart.o(i.drv_uart_recv_none_blocking) for drv_uart_recv_none_blocking
    hal_uart.o(i.hal_uart_recv_none_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_send_blocking) refers to drv_uart.o(i.drv_uart_send_blocking) for drv_uart_send_blocking
    hal_uart.o(i.hal_uart_send_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_uart.o(i.hal_uart_send_none_blocking) refers to drv_uart.o(i.drv_uart_send_none_blocking) for drv_uart_send_none_blocking
    hal_uart.o(i.hal_uart_send_none_blocking) refers to hal_uart.o(.constdata) for .constdata
    hal_internal_vsync.o(i.LCDC_IRQn_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.LCDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_internal_vsync.o(i.LCDC_IRQn_Handler) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) for hal_intl_fb_cal_fb_info
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init) for hal_dsi_rx_ctrl_init
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start) for hal_dsi_rx_ctrl_start
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal) for hal_dsi_tx_ctrl_gen_a_tear_signal
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to tau_delay.o(i.delayUs) for delayUs
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) for hal_vsync_reset_lcdc_scaler
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_sync_register_rx_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) for hal_intl_fb_set_fb_info_manual
    hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_deinit) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) for hal_intl_fb_cal_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_svs.o(i.hal_intl_svs_init_rx) for hal_intl_svs_init_rx
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr) for hal_intl_dcs_init_sw_fltr
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_rxbr.o(i.drv_rxbr_register_irq1_callback) for drv_rxbr_register_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to drv_vidc.o(i.drv_vidc_register_callback) for drv_vidc_register_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_init) for dcs_packet_fifo_init
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_pro_motion_init) for soft_pro_motion_init
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_gen_te) for soft_gen_te
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.rxbr_irq1_callback) for rxbr_irq1_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.vidc_callback) for vidc_callback
    hal_internal_vsync.o(i.hal_internal_vsync_init_rx) refers to hal_internal_vsync.o(i.soft_gen_te_double_buffer) for soft_gen_te_double_buffer
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(i.check_mipi_rx_tx_video_info) for check_mipi_rx_tx_video_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) for hal_intl_fb_cal_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_init_tx) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_svs.o(i.hal_intl_svs_deinit_rx) for hal_intl_svs_deinit_rx
    hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_svs.o(i.hal_intl_svs_set_sync_coef) for hal_intl_svs_set_sync_coef
    hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_config_int_single) for drv_lcdc_config_int_single
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_memc.o(i.drv_memc_set_frame_drop_select) for drv_memc_set_frame_drop_select
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_memc.o(i.drv_memc_set_tear_mode) for drv_memc_set_tear_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line) for hal_internal_vsync_get_sync_line
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_set_tear_line) for drv_lcdc_set_tear_line
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to drv_lcdc.o(i.drv_lcdc_config_acc_command_mode) for drv_lcdc_config_acc_command_mode
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.hal_internal_vsync_deinit) for hal_internal_vsync_deinit
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_svs.o(i.hal_intl_svs_deinit_tx) for hal_intl_svs_deinit_tx
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(i.soft_pro_motion_init) for soft_pro_motion_init
    hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_internal_svs.o(i.hal_intl_svs_set_input_frate) for hal_intl_svs_set_input_frate
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_rate_transfer_sel) for drv_memc_rate_transfer_sel
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_memc.o(i.drv_memc_sel_vsync) for drv_memc_sel_vsync
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg) for drv_rxbr_hline_rcv0_cfg
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dadd.o(.text) for __aeabi_dadd
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_internal_vsync.o(i.soft_pro_motion_init) for soft_pro_motion_init
    hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.drv_rxbr_get_int_source) for drv_rxbr_get_int_source
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.soft_double_buffer_update) for soft_double_buffer_update
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_svs.o(i.hal_intl_svs_handle) for hal_intl_svs_handle
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(i.vpre_err_reset) for vpre_err_reset
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_vidc.o(i.drv_vidc_enable) for drv_vidc_enable
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs) for drv_dsi_tx_phy_clock_lane_req_hs
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_lcdc.o(i.drv_lcdc_cmd_start) for drv_lcdc_cmd_start
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt) for hal_intl_svs_set_rx_vtt
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.rxbr_irq1_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.soft_double_buffer_update) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(i.soft_tear_adjust_line) for soft_tear_adjust_line
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_gen_te) refers to hal_internal_vsync.o(.data) for .data
    hal_internal_vsync.o(i.soft_gen_te_double_buffer) refers to hal_internal_vsync.o(i.soft_tear_adjust_line) for soft_tear_adjust_line
    hal_internal_vsync.o(i.soft_gen_te_double_buffer) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_pro_motion_init) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_vsync.o(i.soft_pro_motion_init) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.soft_pro_motion_init) refers to hal_internal_fb.o(.bss) for g_rx_fb_info
    hal_internal_vsync.o(i.soft_tear_adjust_line) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_get_int_source) for drv_vidc_get_int_source
    hal_internal_vsync.o(i.vidc_callback) refers to drv_lcdc.o(i.drv_lcdc_function_disable) for drv_lcdc_function_disable
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_set_irqen) for drv_vidc_set_irqen
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_clear_irq) for drv_vidc_clear_irq
    hal_internal_vsync.o(i.vidc_callback) refers to drv_vidc.o(i.drv_vidc_get_irq_status) for drv_vidc_get_irq_status
    hal_internal_vsync.o(i.vidc_callback) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_vsync.o(i.vidc_callback) refers to hal_internal_vsync.o(.conststring) for .conststring
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    hal_internal_vsync.o(i.vpre_err_reset) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    hal_internal_vsync.o(i.vpre_err_reset) refers to hal_internal_vsync.o(.bss) for .bss
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to hal_internal_dcs.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) for hal_intl_dcs_rx_receive_packet
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_dsc_dec.o(i.drv_dsc_dec_get_nslc) for drv_dsc_dec_get_nslc
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_crgu.o(i.drv_crgu_set_dsc_clk) for drv_crgu_set_dsc_clk
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    hal_internal_dcs.o(i.VPRE_IRQn_Handler) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to hal_internal_dcs.o(i.drv_rxbr_get_status0) for drv_rxbr_get_status0
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_dcs.o(i.check_pkt_buf_rev) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr) refers to hal_internal_dcs.o(.bss) for .bss
    hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_register_write_cmd_entry) refers to hal_internal_dcs.o(.data) for .data
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle) for hal_intl_dcs_sw_filter_handle
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) for dcs_packet_fifo_alloc
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler) for hal_dsi_rx_ctrl_dcs_async_handler
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_ddi_crc_en) for drv_dsi_rx_get_ddi_crc_en
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_dcs.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload) for drv_dsi_tx_command_put_payload
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_dcs.o(.data) for .data
    hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) refers to hal_internal_dcs.o(.conststring) for .conststring
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data) for hal_intl_dcs_rx_get_dcs_packet_data
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) for hal_intl_dcs_rx_receive_pps
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer) for drv_rxbr_clear_pkt_buffer
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to hal_internal_dcs.o(i.check_pkt_buf_rev) for check_pkt_buf_rev
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en) for drv_dsi_rx_get_compression_en
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to drv_dsc_dec.o(i.drv_dsc_dec_enable) for drv_dsc_dec_enable
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to hal_internal_dcs.o(.conststring) for .conststring
    hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) refers to memseta.o(.text) for __aeabi_memset
    hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) refers to drv_rxbr.o(i.drv_rxbr_set_filter_regs) for drv_rxbr_set_filter_regs
    hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) refers to hal_internal_dcs.o(.bss) for .bss
    hal_internal_dcs.o(i.hal_intl_dcs_set_dcs_direct_mode) refers to hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter) for hal_intl_dcs_set_auto_hw_filter
    hal_internal_dcs.o(i.hal_intl_dcs_set_dcs_direct_mode) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle) refers to hal_internal_dcs.o(.data) for .data
    hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle) refers to hal_internal_dcs.o(.bss) for .bss
    hal_internal_dcs.o(.data) refers to hal_internal_dcs.o(.bss) for g_imm_buffer
    hal_internal_fb.o(i.ha_intl_fb_check_pu_size) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.ha_intl_fb_check_pu_size) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter) for hal_intl_fb_flow_control_adapter
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) for hal_intl_fb_check_bandwidth
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.ha_intl_fb_check_pu_size) for ha_intl_fb_check_pu_size
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(i.hal_intl_fb_edge_resize) for hal_intl_fb_edge_resize
    hal_internal_fb.o(i.hal_intl_fb_cal_fb_info) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) refers to hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode) for hal_internal_sync_get_hight_performan_mode
    hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.hal_intl_fb_check_bandwidth) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_fb.o(i.hal_intl_fb_edge_resize) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.hal_intl_fb_edge_resize) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) refers to memcpya.o(.text) for __aeabi_memcpy4
    hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_get_user_flow) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to hal_internal_fb.o(.bss) for .bss
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to hal_internal_vsync.o(.bss) for g_vsync_handle
    hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual) refers to hal_internal_fb.o(.conststring) for .conststring
    hal_internal_svs.o(i.hal_intl_svs_deinit_rx) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.hal_intl_svs_deinit_rx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_deinit_rx) refers to hal_internal_svs.o(i.svs_wait_start) for svs_wait_start
    hal_internal_svs.o(i.hal_intl_svs_deinit_tx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_handle) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to memseta.o(.text) for __aeabi_memclr4
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) for hal_intl_svs_update_rxbr_clk
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_fb.o(i.hal_intl_fb_get_user_flow) for hal_intl_fb_get_user_flow
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_init_rx) refers to hal_internal_svs.o(i.svs_wait_start) for svs_wait_start
    hal_internal_svs.o(i.hal_intl_svs_init_tx) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_svs.o(i.svs_wait_start) for svs_wait_start
    hal_internal_svs.o(i.hal_intl_svs_set_input_frate) refers to hal_internal_svs.o(i.svs_wait_fr_stab) for svs_wait_fr_stab
    hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_set_sync_coef) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to dfltui.o(.text) for __aeabi_ui2d
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to dmul.o(.text) for __aeabi_dmul
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info) for hal_intl_fb_get_rx_fb_info
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg) for drv_rxbr_hline_rcv1_cfg
    hal_internal_svs.o(i.svs_direct_mode_setting) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_get_rel_intv) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_svs.o(i.svs_get_rel_intv) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_sync_handle) refers to hal_internal_svs.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_svs.o(i.svs_sync_handle) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_svs.o(i.svs_sync_handle) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_svs.o(i.svs_sync_handle) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_svs.o(i.svs_sync_handle) refers to f2d.o(.text) for __aeabi_f2d
    hal_internal_svs.o(i.svs_sync_handle) refers to dadd.o(.text) for __aeabi_dadd
    hal_internal_svs.o(i.svs_sync_handle) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_svs.o(i.svs_sync_handle) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to hal_internal_svs.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to drv_rxbr.o(i.drv_rxbr_frame_drop_cfg) for drv_rxbr_frame_drop_cfg
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to uidiv.o(.text) for __aeabi_uidivmod
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to ffixui.o(.text) for __aeabi_f2uiz
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_wait_fr_stab) refers to hal_internal_svs.o(i.svs_sync_handle) for svs_sync_handle
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(i.svs_get_rel_intv) for svs_get_rel_intv
    hal_internal_svs.o(i.svs_wait_start) refers to drv_crgu.o(i.drv_crgu_get_rxbr_clk) for drv_crgu_get_rxbr_clk
    hal_internal_svs.o(i.svs_wait_start) refers to ffltui.o(.text) for __aeabi_ui2f
    hal_internal_svs.o(i.svs_wait_start) refers to fdiv.o(.text) for __aeabi_fdiv
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state) for hal_internal_vsync_get_tx_state
    hal_internal_svs.o(i.svs_wait_start) refers to fmul.o(.text) for __aeabi_fmul
    hal_internal_svs.o(i.svs_wait_start) refers to f2d.o(.text) for __aeabi_f2d
    hal_internal_svs.o(i.svs_wait_start) refers to ceil.o(i.ceil) for ceil
    hal_internal_svs.o(i.svs_wait_start) refers to dfixui.o(.text) for __aeabi_d2uiz
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(i.svs_direct_mode_setting) for svs_direct_mode_setting
    hal_internal_svs.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_clear_status0) for drv_rxbr_clear_status0
    hal_internal_svs.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_set_inten) for drv_rxbr_set_inten
    hal_internal_svs.o(i.svs_wait_start) refers to drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg) for drv_rxbr_hline_rcv1_cfg
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(.bss) for .bss
    hal_internal_svs.o(i.svs_wait_start) refers to hal_internal_svs.o(i.svs_wait_fr_stab) for svs_wait_fr_stab
    drv_common.o(i.HardFault_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_common.o(i.SysTick_Handler) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_enable_systick) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_common.o(i.drv_common_enable_systick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_get_tick) refers to drv_common.o(.data) for .data
    drv_common.o(i.drv_common_system_init) refers to drv_se.o(i.drv_se_init) for drv_se_init
    drv_common.o(i.drv_common_systick_register_cb) refers to drv_common.o(.data) for .data
    drv_crgu.o(i.drv_crgu_get_rxbr_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_crgu.o(i.drv_crgu_get_system_clk) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(i.drv_dma_get_int_source) for drv_dma_get_int_source
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(i.drv_dma_clear_status) for drv_dma_clear_status
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.DMA_IRQn_Handler) refers to drv_dma.o(.data) for .data
    drv_dma.o(i.drv_dma_apply_handle) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dma.o(i.drv_dma_apply_handle) refers to drv_dma.o(.data) for .data
    drv_dma.o(i.drv_dma_apply_handle) refers to drv_dma.o(.constdata) for .constdata
    drv_dma.o(i.drv_dma_deinit) refers to drv_dma.o(i.drv_dma_disable_int) for drv_dma_disable_int
    drv_dma.o(i.drv_dma_disable_int) refers to drv_dma.o(i.drv_dma_int_list_delete) for drv_dma_int_list_delete
    drv_dma.o(i.drv_dma_disable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dma.o(i.drv_dma_enable_int) refers to drv_dma.o(i.drv_dma_int_list_inset) for drv_dma_int_list_inset
    drv_dma.o(i.drv_dma_enable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dma.o(i.drv_dma_init) refers to drv_per_common.o(i.drv_per_set_clock) for drv_per_set_clock
    drv_dma.o(i.drv_dma_init) refers to drv_dma.o(i.drv_dma_update_handle_setting) for drv_dma_update_handle_setting
    drv_dma.o(i.drv_dma_int_list_delete) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_int_list_inset) refers to drv_dma.o(.bss) for .bss
    drv_dma.o(i.drv_dma_update_handle_setting) refers to drv_sys_cfg.o(i.drv_sys_cfg_sel_dma_req) for drv_sys_cfg_sel_dma_req
    drv_dma.o(i.drv_dma_update_req_by_default) refers to drv_dma.o(i.drv_dma_update_handle_setting) for drv_dma_update_handle_setting
    drv_dma.o(i.drv_dma_update_req_by_default) refers to drv_dma.o(.constdata) for .constdata
    drv_dsc_dec.o(i.drv_dsc_dec_enable) refers to drv_se.o(i.drv_se_set_dsc) for drv_se_set_dsc
    drv_gpio.o(i.AP_NRESET_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.AP_NRESET_IRQn_Handler) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.EXTI_INT0_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT1_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT2_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT3_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT4_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT5_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT6_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.EXTI_INT7_IRQn_Handler) refers to drv_gpio.o(i.drv_gpio_handle_int) for drv_gpio_handle_int
    drv_gpio.o(i.drv_gpio_handle_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_gpio.o(i.drv_gpio_handle_int) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_register_ap_reset_callback) refers to drv_gpio.o(.data) for .data
    drv_gpio.o(i.drv_gpio_register_callback) refers to drv_gpio.o(.bss) for .bss
    drv_gpio.o(i.drv_gpio_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_pwr.o(i.drv_pwr_analog_pwm_en) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_elvcc_pwm_en) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_elvcc_pwm_en) refers to tau_delay.o(i.delayMs) for delayMs
    drv_pwr.o(i.drv_pwr_enter_sleep_mode) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_enter_sleep_mode) refers to drv_pwr.o(i.drv_pwr_por_mode_flag) for drv_pwr_por_mode_flag
    drv_pwr.o(i.drv_pwr_enter_stop_sleep_mode) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_exit_sleep_mode) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_hv_ldo_mode_clock_sel) refers to drv_pwr.o(i.drv_pwr_hv_ldo_10M_clock) for drv_pwr_hv_ldo_10M_clock
    drv_pwr.o(i.drv_pwr_pwm_output_pwm_led) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_breath_screen_power_sel) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_digit_power_sel) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_system_clk) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_pwr.o(i.drv_pwr_set_wakeup_type) refers to drv_pwr.o(i.drv_pwr_write_lock) for drv_pwr_write_lock
    drv_spi_master.o(i.drv_spim_disable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_spi_master.o(i.drv_spim_disable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_spi_master.o(i.drv_spim_enable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_spi_master.o(i.drv_spim_enable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_spi_master.o(i.drv_spim_init) refers to drv_per_common.o(i.drv_per_get_system_clk) for drv_per_get_system_clk
    drv_spi_master.o(i.drv_spim_init) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_swire.o(i.SWIRE_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_swire.o(i.SWIRE_IRQn_Handler) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_register_callback) refers to drv_swire.o(.data) for .data
    drv_swire.o(i.drv_swire_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_sys_cfg.o(i.drv_sys_cfg_sel_dma_req) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_timer.o(i.TIMER0_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.TIMER1_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.TIMER2_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.TIMER3_IRQn_Handler) refers to drv_timer.o(i.drv_timer_handle_interrupt) for drv_timer_handle_interrupt
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_clear_status_flags) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_timer.o(i.drv_timer_enable) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_get_instance) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_get_status) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_clear_status_flags) for drv_timer_clear_status_flags
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_int) for drv_timer_set_int
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(i.drv_timer_set_compare_val) for drv_timer_set_compare_val
    drv_timer.o(i.drv_timer_handle_interrupt) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_register_callback) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_compare_val) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_compare_val) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_timer.o(i.drv_timer_set_compare_val) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_compare_val) refers to drv_common.o(.data) for g_system_clock
    drv_timer.o(i.drv_timer_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(i.drv_timer_get_instance) for drv_timer_get_instance
    drv_timer.o(i.drv_timer_set_prescaler) refers to drv_timer.o(.data) for .data
    drv_timer.o(i.drv_timer_set_repeat) refers to drv_timer.o(.data) for .data
    drv_wdg.o(i.WDG_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_wdg.o(i.WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_set_int) for drv_wdg_set_int
    drv_wdg.o(i.WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_clear_counter) for drv_wdg_clear_counter
    drv_wdg.o(i.WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_read_edge_flag) for drv_wdg_read_edge_flag
    drv_wdg.o(i.WDG_IRQn_Handler) refers to drv_wdg.o(i.drv_wdg_clear_edge_flag) for drv_wdg_clear_edge_flag
    drv_wdg.o(i.WDG_IRQn_Handler) refers to drv_wdg.o(.data) for .data
    drv_wdg.o(i.drv_wdg_register_callback) refers to drv_wdg.o(.data) for .data
    drv_wdg.o(i.drv_wdg_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_wdg.o(i.drv_wdg_set_repeat) refers to drv_wdg.o(.data) for .data
    drv_crc.o(i.drv_crc_write_data_register) refers to drv_crc.o(i.drv_crc_get_tcrc_register) for drv_crc_get_tcrc_register
    drv_i2c.o(i.I2C0_IRQn_Handler) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.I2C1_IRQn_Handler) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.I2C2_IRQn_Handler) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_NVIC_enable) refers to drv_i2c.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_i2c.o(i.drv_i2c_NVIC_enable) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_clear_intr_status) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_i2c.o(i.drv_i2c_clear_intr_status) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_clock_enable) refers to drv_per_common.o(i.drv_per_set_clock) for drv_per_set_clock
    drv_i2c.o(i.drv_i2c_clock_enable) refers to drv_i2c.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_i2c.o(i.drv_i2c_clock_enable) refers to drv_per_common.o(i.drv_per_reset_module) for drv_per_reset_module
    drv_i2c.o(i.drv_i2c_clock_enable) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_disable_dma_req) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_disable_intr) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_enable) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_enable_dma_req) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_enable_intr) refers to drv_i2c.o(i.drv_i2c_set_sys_mask) for drv_i2c_set_sys_mask
    drv_i2c.o(i.drv_i2c_enable_intr) refers to drv_i2c.o(i.drv_i2c_clear_intr_status) for drv_i2c_clear_intr_status
    drv_i2c.o(i.drv_i2c_enable_intr) refers to drv_i2c.o(i.drv_i2c_NVIC_enable) for drv_i2c_NVIC_enable
    drv_i2c.o(i.drv_i2c_enable_intr) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_flush) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_get_fifo_status) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_get_intr_status) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_get_rx_count) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_get_tx_abrtsource) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_read_data) refers to drv_i2c.o(i.drv_i2c_get_fifo_status) for drv_i2c_get_fifo_status
    drv_i2c.o(i.drv_i2c_read_data) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_set_callback) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_set_fifo_threshold) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_set_sys_mask) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_i2c.o(i.drv_i2c_set_sys_mask) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_i2c.o(i.drv_i2c_set_sys_mask) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2c_write_data) refers to drv_i2c.o(i.drv_i2c_get_fifo_status) for drv_i2c_get_fifo_status
    drv_i2c.o(i.drv_i2c_write_data) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cm_cal_scl_cnt) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_i2c.o(i.drv_i2cm_cal_scl_cnt) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cm_init) refers to drv_per_common.o(i.drv_per_get_system_clk) for drv_per_get_system_clk
    drv_i2c.o(i.drv_i2cm_init) refers to drv_i2c.o(i.drv_i2cm_cal_scl_cnt) for drv_i2cm_cal_scl_cnt
    drv_i2c.o(i.drv_i2cm_init) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cm_multi_params_read_data) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cm_read_data) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cm_set_baud_rate) refers to drv_per_common.o(i.drv_per_get_system_clk) for drv_per_get_system_clk
    drv_i2c.o(i.drv_i2cm_set_baud_rate) refers to drv_i2c.o(i.drv_i2cm_cal_scl_cnt) for drv_i2cm_cal_scl_cnt
    drv_i2c.o(i.drv_i2cm_set_baud_rate) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cm_set_slave_addr) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cm_write_data) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cm_write_read_cmd) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cs_init) refers to drv_i2c.o(.data) for .data
    drv_i2c.o(i.drv_i2cs_own_addr) refers to drv_i2c.o(.data) for .data
    drv_per_common.o(i.drv_per_get_system_clk) refers to drv_crgu.o(i.drv_crgu_get_system_clk) for drv_crgu_get_system_clk
    drv_per_common.o(i.drv_per_reset_module) refers to drv_crgu.o(i.drv_crgu_reset_modules) for drv_crgu_reset_modules
    drv_per_common.o(i.drv_per_set_clock) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    dcs_packet_fifo.o(i.dcs_packet_fifo_alloc) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_fifo_init) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_free_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_header) refers to dcs_packet_fifo.o(.bss) for .bss
    dcs_packet_fifo.o(i.dcs_packet_get_fifo_size) refers to dcs_packet_fifo.o(.bss) for .bss
    drv_se.o(i.drv_se_init) refers to drv_efuse.o(i.drv_efuse_enter_inactive) for drv_efuse_enter_inactive
    drv_se.o(i.drv_se_init) refers to drv_efuse.o(i.drv_efuse_read) for drv_efuse_read
    drv_se.o(i.drv_se_init) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_dsc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_dsc) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_lcdc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_lcdc) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_memc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_memc) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_rxbr) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_rxbr) refers to drv_se.o(.data) for .data
    drv_se.o(i.drv_se_set_vidc) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_se.o(i.drv_se_set_vidc) refers to drv_se.o(.data) for .data
    drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler) refers to drv_dsi_rx.o(.data) for .data
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) for drv_dsi_rx_get_color_bpp
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to ffltui.o(.text) for __aeabi_ui2f
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fdiv.o(.text) for __aeabi_fdiv
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fmul.o(.text) for __aeabi_fmul
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc) for drv_dsi_rx_get_color_pcc
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to fadd.o(.text) for __aeabi_fadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to cfrcmple.o(.text) for __aeabi_cfrcmple
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to f2d.o(.text) for __aeabi_f2d
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dadd.o(.text) for __aeabi_dadd
    drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay) refers to dfixui.o(.text) for __aeabi_d2uiz
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_rx.o(i.drv_dsi_rx_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_rx.o(i.drv_dsi_rx_set_drv_log_level) refers to drv_dsi_rx.o(.data) for .data
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy) refers to drv_phy_common.o(i.drv_phy_test_lock) for drv_phy_test_lock
    drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_enter) for drv_tx_phy_test_enter
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_phy_common.o(i.drv_phy_test_clear) for drv_phy_test_clear
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_write_code) for drv_tx_phy_test_write_code
    drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup) refers to drv_dsi_tx.o(i.drv_tx_phy_test_exit) for drv_tx_phy_test_exit
    drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate) for drv_dsi_tx_phy_status_stopstate
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to tau_log.o(i.tau_log_printf) for tau_log_printf
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot) for drv_dsi_tx_phy_status_ulpsactivenot
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock) for drv_dsi_tx_phy_status_pll_lock
    drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit) refers to drv_dsi_tx.o(i.drv_dsi_tx_version) for drv_dsi_tx_version
    drv_dsi_tx.o(i.drv_dsi_tx_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_dsi_tx.o(i.drv_dsi_tx_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_lcdc.o(i.drv_lcdc_clear_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_lcdc.o(i.drv_lcdc_cmd_start) refers to drv_se.o(i.drv_se_set_lcdc) for drv_se_set_lcdc
    drv_lcdc.o(i.drv_lcdc_ctrl_flow) refers to drv_lcdc.o(i.drv_lcdc_function_enable) for drv_lcdc_function_enable
    drv_lcdc.o(i.drv_lcdc_part_display_config) refers to drv_lcdc.o(i.drv_lcdc_pixel_value_config) for drv_lcdc_pixel_value_config
    drv_lcdc.o(i.drv_lcdc_set_int) refers to drv_lcdc.o(i.drv_lcdc_clear_int) for drv_lcdc_clear_int
    drv_lcdc.o(i.drv_lcdc_set_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_lcdc.o(i.drv_lcdc_vid_hw_start) refers to drv_se.o(i.drv_se_set_lcdc) for drv_se_set_lcdc
    drv_memc.o(i.MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_get_status) for drv_memc_get_status
    drv_memc.o(i.MEMC_IRQn_Handler) refers to drv_memc.o(i.drv_memc_clear_status) for drv_memc_clear_status
    drv_memc.o(i.MEMC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_memc.o(i.drv_memc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_memc.o(i.drv_memc_rate_transfer_sel) refers to drv_se.o(i.drv_se_set_memc) for drv_se_set_memc
    drv_memc.o(i.drv_memc_set_ltpo_mode) refers to drv_se.o(i.drv_se_set_memc) for drv_se_set_memc
    drv_rxbr.o(i.VPRE1_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.VPRE1_IRQn_Handler) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_EnableIRQ) for __NVIC_EnableIRQ
    drv_rxbr.o(i.drv_rxbr_enable_irq) refers to drv_rxbr.o(i.__NVIC_DisableIRQ) for __NVIC_DisableIRQ
    drv_rxbr.o(i.drv_rxbr_register_irq0_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_register_irq1_callback) refers to drv_rxbr.o(.data) for .data
    drv_rxbr.o(i.drv_rxbr_set_cmd_filter) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_rxbr.o(i.drv_rxbr_set_cmd_response) refers to hal_dsi_rx_ctrl.o(i.__ARM_common_switch8) for __ARM_common_switch8
    drv_rxbr.o(i.drv_rxbr_set_color_format) refers to drv_se.o(i.drv_se_set_rxbr) for drv_se_set_rxbr
    drv_rxbr.o(i.drv_rxbr_soft_reset) refers to tau_delay.o(i.delayMs) for delayMs
    drv_rxbr.o(i.drv_rxbr_sw_reset) refers to drv_crgu.o(i.drv_crgu_set_reset) for drv_crgu_set_reset
    drv_rxbr.o(i.drv_rxbr_sw_reset) refers to drv_vidc.o(i.drv_vidc_reset) for drv_vidc_reset
    drv_vidc.o(i.VIDC_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.VIDC_IRQn_Handler) refers to drv_vidc.o(.data) for .data
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_vidc.o(i.drv_vidc_enable_irq) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_vidc.o(i.drv_vidc_register_callback) refers to drv_vidc.o(.data) for .data
    drv_vidc.o(i.drv_vidc_set_src_parameter) refers to drv_se.o(i.drv_se_set_vidc) for drv_se_set_vidc
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_int_trans_handle) for drv_uart_int_trans_handle
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_abort_recv) for drv_uart_abort_recv
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(i.drv_uart_abort_send) for drv_uart_abort_send
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_sys_cfg.o(i.drv_sys_cfg_clear_pending) for drv_sys_cfg_clear_pending
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(.constdata) for .constdata
    drv_uart.o(i.UART_IRQn_Handler) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(i.drv_uart_reset_rx_fifo) for drv_uart_reset_rx_fifo
    drv_uart.o(i.drv_uart_abort_recv) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(i.drv_uart_reset_tx_fifo) for drv_uart_reset_tx_fifo
    drv_uart.o(i.drv_uart_abort_send) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_deinit) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_deinit) refers to drv_uart.o(i.drv_uart_enable_clk) for drv_uart_enable_clk
    drv_uart.o(i.drv_uart_deinit) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.drv_uart_deinit) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_enable_clk) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    drv_uart.o(i.drv_uart_enable_int) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_enable_int) refers to drv_sys_cfg.o(i.drv_sys_cfg_set_int) for drv_sys_cfg_set_int
    drv_uart.o(i.drv_uart_get_def_cfg) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.drv_uart_get_def_cfg) refers to drv_common.o(.data) for g_system_clock
    drv_uart.o(i.drv_uart_get_instance) refers to drv_uart.o(.constdata) for .constdata
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_enable_clk) for drv_uart_enable_clk
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_set_baud_rate) for drv_uart_set_baud_rate
    drv_uart.o(i.drv_uart_init) refers to drv_uart.o(i.drv_uart_enable_int) for drv_uart_enable_int
    drv_uart.o(i.drv_uart_int_trans_handle) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_recv_none_blocking) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_recv_none_blocking) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_recv_none_blocking) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_reset_rx_fifo) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_reset_tx_fifo) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_send_none_blocking) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_send_none_blocking) refers to drv_uart.o(i.drv_uart_config_int) for drv_uart_config_int
    drv_uart.o(i.drv_uart_send_none_blocking) refers to drv_uart.o(.bss) for .bss
    drv_uart.o(i.drv_uart_set_baud_rate) refers to uidiv.o(.text) for __aeabi_uidivmod
    drv_uart.o(i.drv_uart_trans_create_handle) refers to drv_uart.o(i.drv_uart_get_instance) for drv_uart_get_instance
    drv_uart.o(i.drv_uart_trans_create_handle) refers to memseta.o(.text) for __aeabi_memclr4
    drv_uart.o(i.drv_uart_trans_create_handle) refers to drv_uart.o(.bss) for .bss
    drv_efuse.o(i.drv_efuse_enter_inactive) refers to drv_crgu.o(i.drv_crgu_enable_clock) for drv_crgu_enable_clock
    drv_efuse.o(i.drv_efuse_enter_inactive) refers to drv_efuse.o(i.drv_efuse_int_enable) for drv_efuse_int_enable
    drv_efuse.o(i.drv_efuse_read) refers to drv_pwr.o(i.drv_pwr_efuse_pd) for drv_pwr_efuse_pd
    drv_efuse.o(i.drv_efuse_read) refers to drv_efuse.o(i.drv_efuse_read_req) for drv_efuse_read_req
    drv_efuse.o(i.drv_efuse_write) refers to drv_pwr.o(i.drv_pwr_efuse_pd) for drv_pwr_efuse_pd
    drv_efuse.o(i.drv_efuse_write) refers to drv_efuse.o(i.drv_efuse_write_req) for drv_efuse_write_req
    drv_efuse.o(i.drv_efuse_write_read_req_clear) refers to drv_efuse.o(i.drv_efuse_write_req) for drv_efuse_write_req
    drv_efuse.o(i.drv_efuse_write_read_req_clear) refers to drv_efuse.o(i.drv_efuse_read_req) for drv_efuse_read_req
    ceil.o(i.__softfp_ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.__softfp_ceil) refers to ceil.o(i.ceil) for ceil
    ceil.o(i.ceil) refers (Special) to iusefp.o(.text) for __I$use$fp
    ceil.o(i.ceil) refers to dadd.o(.text) for __aeabi_dadd
    ceil.o(i.ceil) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry10a.o(.ARM.Collect$$$$0000000D) for __rt_final_cpp
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry11a.o(.ARM.Collect$$$$0000000F) for __rt_final_exit
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry7b.o(.ARM.Collect$$$$00000008) for _main_clock
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry8b.o(.ARM.Collect$$$$0000000A) for _main_cpp_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry9a.o(.ARM.Collect$$$$0000000B) for _main_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry5.o(.ARM.Collect$$$$00000004) for _main_scatterload
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry2.o(.ARM.Collect$$$$00000001) for _main_stk
    idiv.o(.text) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfb.o(i.__0fprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0fprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0printf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printfb.o(i.__0vfprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vfprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vprintf$bare) refers to tau_log.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printf0.o(i.__0fprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0fprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0printf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf0.o(i.__0vfprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vfprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vprintf$0) refers to tau_log.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf1.o(i.__0fprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0fprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0printf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i.__0vfprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vfprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vprintf$1) refers to tau_log.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf2.o(i.__0fprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0fprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0printf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf2.o(i.__0vfprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vfprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vprintf$2) refers to tau_log.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf3.o(i.__0fprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0fprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0printf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i.__0vfprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vfprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vprintf$3) refers to tau_log.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf4.o(i.__0fprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0fprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0printf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i.__0vfprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vfprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vprintf$4) refers to tau_log.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf5.o(i.__0fprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0fprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0printf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i.__0vfprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vfprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vprintf$5) refers to tau_log.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf6.o(i.__0fprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0fprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0printf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i.__0vfprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vfprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vprintf$6) refers to tau_log.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i._printf_core) refers to printf6.o(i._printf_pre_padding) for _printf_pre_padding
    printf6.o(i._printf_core) refers to printf6.o(i._printf_post_padding) for _printf_post_padding
    printf6.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf7.o(i.__0fprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0fprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0printf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i.__0vfprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vfprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vprintf$7) refers to tau_log.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i._printf_core) refers to printf7.o(i._printf_pre_padding) for _printf_pre_padding
    printf7.o(i._printf_core) refers to printf7.o(i._printf_post_padding) for _printf_post_padding
    printf7.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf8.o(i.__0fprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0fprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0printf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i.__0vfprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vfprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vprintf$8) refers to tau_log.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i._printf_core) refers to printf8.o(i._printf_pre_padding) for _printf_pre_padding
    printf8.o(i._printf_core) refers to printf8.o(i._printf_post_padding) for _printf_post_padding
    printf8.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i.__0fprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0fprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0fprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0printf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0printf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0snprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0snprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0snprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0sprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0sprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0sprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i.__0vfprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vfprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vfprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vprintf) refers to tau_log.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0vsnprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0vsprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i._fp_digits) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._fp_digits) refers to dmul.o(.text) for __aeabi_dmul
    printfa.o(i._fp_digits) refers to ddiv.o(.text) for __aeabi_ddiv
    printfa.o(i._fp_digits) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    printfa.o(i._fp_digits) refers to dadd.o(.text) for __aeabi_dadd
    printfa.o(i._fp_digits) refers to dfixul.o(.text) for __aeabi_d2ulz
    printfa.o(i._fp_digits) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_core) refers to printfa.o(i._printf_pre_padding) for _printf_pre_padding
    printfa.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers to printfa.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i._printf_core) refers to printfa.o(i._fp_digits) for _fp_digits
    printfa.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfa.o(i._printf_post_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_pre_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._snputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._sputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fadd.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    fmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    fdiv.o(.text) refers to fepilogue.o(.text) for _float_round
    fscalb.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dadd.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    dadd.o(.text) refers to llsshr.o(.text) for __aeabi_lasr
    dadd.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dmul.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ddiv.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ddiv.o(.text) refers to depilogue.o(.text) for _double_round
    ffltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ffltui.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    dfltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfltui.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ffixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    dfixui.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    f2d.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    d2f.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    d2f.o(.text) refers to fepilogue.o(.text) for _float_round
    cfcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    cfrcmple.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    entry2.o(.ARM.Collect$$$$00000001) refers to entry2.o(.ARM.Collect$$$$00002712) for __lit__00000000
    entry2.o(.ARM.Collect$$$$00002712) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to startup_armcm0.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    entry5.o(.ARM.Collect$$$$00000004) refers to init.o(.text) for __scatterload
    entry9a.o(.ARM.Collect$$$$0000000B) refers to main.o(i.main) for main
    entry9b.o(.ARM.Collect$$$$0000000C) refers to main.o(i.main) for main
    uldiv.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    uldiv.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to depilogue.o(i.__ARM_clz) for __ARM_clz
    depilogue.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixul.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixul.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    init.o(.text) refers to entry5.o(.ARM.Collect$$$$00000004) for __main_after_scatterload


==============================================================================

Removing Unused input sections from the image.

    Removing main.o(.rev16_text), (4 bytes).
    Removing main.o(.revsh_text), (4 bytes).
    Removing app_tp_transfer.o(.rev16_text), (4 bytes).
    Removing app_tp_transfer.o(.revsh_text), (4 bytes).
    Removing app_tp_transfer.o(i.app_tp_i2cs_callback), (76 bytes).
    Removing app_tp_transfer.o(i.app_tp_init), (108 bytes).
    Removing app_tp_transfer.o(i.app_tp_m_read), (24 bytes).
    Removing app_tp_transfer.o(i.app_tp_m_transfer_complate), (8 bytes).
    Removing app_tp_transfer.o(i.app_tp_m_write), (28 bytes).
    Removing app_tp_transfer.o(i.app_tp_phone_clear_reset_on), (12 bytes).
    Removing app_tp_transfer.o(i.app_tp_phone_reset_init), (60 bytes).
    Removing app_tp_transfer.o(i.app_tp_phone_reset_on), (12 bytes).
    Removing app_tp_transfer.o(i.app_tp_reset_callback), (12 bytes).
    Removing app_tp_transfer.o(i.app_tp_s_read), (20 bytes).
    Removing app_tp_transfer.o(i.app_tp_s_write), (22 bytes).
    Removing app_tp_transfer.o(i.app_tp_screen_init), (60 bytes).
    Removing app_tp_transfer.o(i.app_tp_screen_int_callback), (12 bytes).
    Removing app_tp_transfer.o(i.app_tp_screen_int_init), (64 bytes).
    Removing app_tp_transfer.o(i.app_tp_screen_int_lvl_low), (28 bytes).
    Removing app_tp_transfer.o(i.app_tp_transfer_phone), (48 bytes).
    Removing app_tp_transfer.o(i.app_tp_transfer_screen_const), (256 bytes).
    Removing app_tp_transfer.o(i.app_tp_transfer_screen_int), (368 bytes).
    Removing app_tp_transfer.o(i.app_tp_transfer_screen_start), (32 bytes).
    Removing app_tp_transfer.o(i.phone_i2cs_io_init), (28 bytes).
    Removing app_tp_transfer.o(i.screen_spim_io_init), (28 bytes).
    Removing app_tp_transfer.o(.bss), (500 bytes).
    Removing app_tp_transfer.o(.constdata), (24 bytes).
    Removing app_tp_transfer.o(.data), (28 bytes).
    Removing app_tp_for_custom_s8.o(.rev16_text), (4 bytes).
    Removing app_tp_for_custom_s8.o(.revsh_text), (4 bytes).
    Removing app_tp_for_custom_s8.o(i.app_tp_phone_analysis_data), (528 bytes).
    Removing app_tp_for_custom_s8.o(i.app_tp_screen_analysis_const), (80 bytes).
    Removing app_tp_for_custom_s8.o(i.app_tp_screen_analysis_int), (1152 bytes).
    Removing app_tp_for_custom_s8.o(i.app_tp_write_other_operations), (60 bytes).
    Removing app_tp_for_custom_s8.o(.bss), (142 bytes).
    Removing app_tp_for_custom_s8.o(.constdata), (1838 bytes).
    Removing app_tp_for_custom_s8.o(.data), (687 bytes).
    Removing s8_demo.o(.rev16_text), (4 bytes).
    Removing s8_demo.o(.revsh_text), (4 bytes).
    Removing s8_demo.o(i.ap_dcs_read), (232 bytes).
    Removing s8_demo.o(i.ap_dcs_set_eye_protection_mode), (100 bytes).
    Removing s8_demo.o(i.ap_rstn_pull_down_cb), (92 bytes).
    Removing s8_demo.o(i.app_mipi_rx_start_cb), (80 bytes).
    Removing board.o(.rev16_text), (4 bytes).
    Removing board.o(.revsh_text), (4 bytes).
    Removing startup_armcm0.o(HEAP), (3072 bytes).
    Removing demo_hal_crc.o(.rev16_text), (4 bytes).
    Removing demo_hal_crc.o(.revsh_text), (4 bytes).
    Removing demo_hal_crc.o(i.demo_crc_array_dma_cal), (44 bytes).
    Removing demo_hal_crc.o(i.demo_crc_dma_callback), (60 bytes).
    Removing demo_hal_crc.o(i.demo_hal_crc_case), (60 bytes).
    Removing demo_hal_crc.o(.constdata), (12 bytes).
    Removing demo_hal_crc.o(.data), (128 bytes).
    Removing demo_hal_dsi_rx.o(.rev16_text), (4 bytes).
    Removing demo_hal_dsi_rx.o(.revsh_text), (4 bytes).
    Removing demo_hal_dsi_rx.o(i.ap_dcs_read), (220 bytes).
    Removing demo_hal_dsi_rx.o(i.cus_dsc_execute), (188 bytes).
    Removing demo_hal_dsi_rx.o(i.demo_hal_dsi_rx_case), (88 bytes).
    Removing demo_hal_dsi_rx.o(i.open_mipi_rx), (200 bytes).
    Removing demo_hal_dsi_rx.o(.constdata), (240 bytes).
    Removing demo_hal_dsi_rx.o(.data), (4 bytes).
    Removing demo_hal_dsi_tx.o(.rev16_text), (4 bytes).
    Removing demo_hal_dsi_tx.o(.revsh_text), (4 bytes).
    Removing demo_hal_dsi_tx.o(i.demo_dsi_tx_case), (68 bytes).
    Removing demo_hal_dsi_tx.o(i.demo_open_mipi_rx), (2 bytes).
    Removing demo_hal_dsi_tx.o(i.demo_open_mipi_tx), (376 bytes).
    Removing demo_hal_dsi_tx.o(i.demo_panel_init), (400 bytes).
    Removing demo_hal_dsi_tx.o(.data), (5 bytes).
    Removing demo_hal_flash.o(.rev16_text), (4 bytes).
    Removing demo_hal_flash.o(.revsh_text), (4 bytes).
    Removing demo_hal_gpio.o(.rev16_text), (4 bytes).
    Removing demo_hal_gpio.o(.revsh_text), (4 bytes).
    Removing demo_hal_i2c.o(.rev16_text), (4 bytes).
    Removing demo_hal_i2c.o(.revsh_text), (4 bytes).
    Removing demo_hal_spi.o(.rev16_text), (4 bytes).
    Removing demo_hal_spi.o(.revsh_text), (4 bytes).
    Removing demo_hal_pwm.o(.rev16_text), (4 bytes).
    Removing demo_hal_pwm.o(.revsh_text), (4 bytes).
    Removing demo_hal_pwr.o(.rev16_text), (4 bytes).
    Removing demo_hal_pwr.o(.revsh_text), (4 bytes).
    Removing demo_hal_swire.o(.rev16_text), (4 bytes).
    Removing demo_hal_swire.o(.revsh_text), (4 bytes).
    Removing demo_hal_uart.o(.rev16_text), (4 bytes).
    Removing demo_hal_uart.o(.revsh_text), (4 bytes).
    Removing demo_hal_wdg.o(.rev16_text), (4 bytes).
    Removing demo_hal_wdg.o(.revsh_text), (4 bytes).
    Removing demo_hal_wdg.o(i.demo_wdg_callback), (72 bytes).
    Removing demo_hal_wdg.o(i.demo_wdg_case), (60 bytes).
    Removing demo_hal_wdg.o(i.demo_wdg_case_int_mode), (196 bytes).
    Removing demo_hal_wdg.o(.data), (3 bytes).
    Removing module_demo_main.o(i.module_demo_main), (2 bytes).
    Removing hal_dsi_rx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_long_cmd), (220 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_ack_short_cmd), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_draw_mode_init), (320 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_enable_test_pattern), (256 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_force_video_crtl), (12 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_compressen_en), (8 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_get_max_ret_size), (32 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_callback), (52 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_register_write_cmd_entry), (10 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_release_handle), (40 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_restart), (68 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_send_ack_cmd), (240 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_hw_filter), (28 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_check_crc), (24 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_cus_esc_clk), (32 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_hw_cmd_filter), (44 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_log_level), (8 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_pixel_data), (240 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rx_clk), (72 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_rxbr_clk), (56 bytes).
    Removing hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_input_frame_rate), (10 bytes).
    Removing hal_dsi_tx_ctrl.o(.rev16_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(.revsh_text), (4 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_cmd_mode), (112 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_draw_flick), (244 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_frame), (12 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_get_disp_line), (12 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_overwrite_enable), (22 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_partial_disp_enable), (70 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_read_cmd), (128 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_release_handle), (32 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_bcs), (60 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_ccm), (8 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_cus_sync_line), (36 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_dect), (60 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_edge_enhance), (60 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_endianness), (12 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_escape_clock_div), (52 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_fc), (60 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_vpg), (28 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_vporch_bta_opera), (68 bytes).
    Removing hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_req_update), (16 bytes).
    Removing hal_gpio.o(.rev16_text), (4 bytes).
    Removing hal_gpio.o(.revsh_text), (4 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_input_data), (18 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_int_type), (20 bytes).
    Removing hal_gpio.o(i.hal_gpio_get_pull_state), (40 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_driving_strength), (44 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_high_impedance), (32 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_pull_state), (72 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_schmitt_trigger), (52 bytes).
    Removing hal_gpio.o(i.hal_gpio_set_slew_rate), (52 bytes).
    Removing hal_i2c_slave.o(.rev16_text), (4 bytes).
    Removing hal_i2c_slave.o(.revsh_text), (4 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_callback), (428 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_deinit), (48 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_get_rx_cnt), (16 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_get_tx_cnt), (16 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_get_write_complete), (20 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_init), (108 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_register_callback), (16 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_rx_cnt_clear), (20 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_set_continue_transfer), (20 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_start), (96 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_stop), (84 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_tx_dma_callback), (56 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_update_rx_buffer), (88 bytes).
    Removing hal_i2c_slave.o(i.hal_i2cs_update_tx_buffer), (80 bytes).
    Removing hal_i2c_slave.o(.data), (160 bytes).
    Removing hal_spi_master.o(.rev16_text), (4 bytes).
    Removing hal_spi_master.o(.revsh_text), (4 bytes).
    Removing hal_spi_master.o(i.hal_spim_deinit), (36 bytes).
    Removing hal_spi_master.o(i.hal_spim_flush), (16 bytes).
    Removing hal_spi_master.o(i.hal_spim_get_transfer_complete), (12 bytes).
    Removing hal_spi_master.o(i.hal_spim_init), (52 bytes).
    Removing hal_spi_master.o(i.hal_spim_read), (56 bytes).
    Removing hal_spi_master.o(i.hal_spim_write), (48 bytes).
    Removing hal_spi_master.o(.data), (4 bytes).
    Removing hal_spi_master.o(.data), (4 bytes).
    Removing hal_swire.o(.rev16_text), (4 bytes).
    Removing hal_swire.o(.revsh_text), (4 bytes).
    Removing hal_swire.o(i.hal_swire_register_callback), (22 bytes).
    Removing hal_swire.o(i.hal_swire_set_waveform), (92 bytes).
    Removing hal_system.o(.rev16_text), (4 bytes).
    Removing hal_system.o(.revsh_text), (4 bytes).
    Removing hal_system.o(i.hal_system_clear_debug_state), (10 bytes).
    Removing hal_system.o(i.hal_system_disable_systick), (8 bytes).
    Removing hal_system.o(i.hal_system_enable_systick), (8 bytes).
    Removing hal_system.o(i.hal_system_get_debug_state), (8 bytes).
    Removing hal_system.o(i.hal_system_get_tick), (8 bytes).
    Removing hal_system.o(i.hal_system_idle_mode), (8 bytes).
    Removing hal_system.o(i.hal_system_register_systick_cb), (8 bytes).
    Removing hal_system.o(i.hal_system_reset_chip), (10 bytes).
    Removing hal_timer.o(.rev16_text), (4 bytes).
    Removing hal_timer.o(.revsh_text), (4 bytes).
    Removing hal_timer.o(i.hal_timer_get_status), (8 bytes).
    Removing hal_timer.o(i.hal_timer_start_ex), (42 bytes).
    Removing hal_wdg.o(.rev16_text), (4 bytes).
    Removing hal_wdg.o(.revsh_text), (4 bytes).
    Removing hal_wdg.o(i.hal_wdg_deinit), (44 bytes).
    Removing hal_wdg.o(i.hal_wdg_init), (12 bytes).
    Removing hal_wdg.o(i.hal_wdg_kick_dog), (20 bytes).
    Removing hal_wdg.o(i.hal_wdg_register_callback), (8 bytes).
    Removing hal_wdg.o(i.hal_wdg_set_repeat), (8 bytes).
    Removing hal_wdg.o(i.hal_wdg_start), (54 bytes).
    Removing hal_wdg.o(i.hal_wdg_stop), (20 bytes).
    Removing hal_crc.o(.rev16_text), (4 bytes).
    Removing hal_crc.o(.revsh_text), (4 bytes).
    Removing hal_crc.o(i.hal_crc_cal), (72 bytes).
    Removing hal_crc.o(i.hal_crc_deinit), (16 bytes).
    Removing hal_crc.o(i.hal_crc_dma_callback), (40 bytes).
    Removing hal_crc.o(i.hal_crc_dma_deinit), (44 bytes).
    Removing hal_crc.o(i.hal_crc_dma_init), (120 bytes).
    Removing hal_crc.o(i.hal_crc_dma_start), (10 bytes).
    Removing hal_crc.o(i.hal_crc_init), (56 bytes).
    Removing hal_crc.o(i.hal_crc_reset), (10 bytes).
    Removing hal_crc.o(.data), (8 bytes).
    Removing hal_pwr.o(.rev16_text), (4 bytes).
    Removing hal_pwr.o(.revsh_text), (4 bytes).
    Removing hal_pwr.o(i.hal_pwr_elvcc_close), (10 bytes).
    Removing hal_pwr.o(i.hal_pwr_elvcc_ldo_en), (46 bytes).
    Removing hal_pwr.o(i.hal_pwr_elvcc_vol_set), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_get_reset_flag), (66 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo13s_en), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo13s_set), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo18s_en), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_ldo18s_set), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_set_pvd), (8 bytes).
    Removing hal_pwr.o(i.hal_pwr_set_vcc_enable), (8 bytes).
    Removing tau_delay.o(.rev16_text), (4 bytes).
    Removing tau_delay.o(.revsh_text), (4 bytes).
    Removing tau_log.o(.rev16_text), (4 bytes).
    Removing tau_log.o(.revsh_text), (4 bytes).
    Removing tau_log.o(i.fgetc), (72 bytes).
    Removing hal_uart.o(.rev16_text), (4 bytes).
    Removing hal_uart.o(.revsh_text), (4 bytes).
    Removing hal_uart.o(i.hal_uart0_rx_dma_cb), (20 bytes).
    Removing hal_uart.o(i.hal_uart0_tx_dma_cb), (36 bytes).
    Removing hal_uart.o(i.hal_uart1_rx_dma_cb), (20 bytes).
    Removing hal_uart.o(i.hal_uart1_tx_dma_cb), (36 bytes).
    Removing hal_uart.o(i.hal_uart_deinit), (48 bytes).
    Removing hal_uart.o(i.hal_uart_dma_path_close), (92 bytes).
    Removing hal_uart.o(i.hal_uart_dma_recv), (276 bytes).
    Removing hal_uart.o(i.hal_uart_dma_send), (280 bytes).
    Removing hal_uart.o(i.hal_uart_recv_blocking), (28 bytes).
    Removing hal_uart.o(i.hal_uart_recv_none_blocking), (28 bytes).
    Removing hal_uart.o(i.hal_uart_send_none_blocking), (28 bytes).
    Removing hal_internal_vsync.o(.rev16_text), (4 bytes).
    Removing hal_internal_vsync.o(.revsh_text), (4 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_cmd_mode_rcv_te), (2 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_register_rx_callback), (28 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_sync_set_fb_setting_manual), (28 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_set_sync_line), (60 bytes).
    Removing hal_internal_vsync.o(i.hal_internal_vsync_toggle_input_frame_rate), (134 bytes).
    Removing hal_internal_vsync.o(.data), (4 bytes).
    Removing hal_internal_dcs.o(.rev16_text), (4 bytes).
    Removing hal_internal_dcs.o(.revsh_text), (4 bytes).
    Removing hal_internal_dcs.o(i.hal_intl_dcs_register_write_cmd_entry), (12 bytes).
    Removing hal_internal_dcs.o(i.hal_intl_dcs_set_dcs_direct_mode), (44 bytes).
    Removing hal_internal_fb.o(.rev16_text), (4 bytes).
    Removing hal_internal_fb.o(.revsh_text), (4 bytes).
    Removing hal_internal_fb.o(i.hal_intl_fb_set_fb_info_manual), (480 bytes).
    Removing hal_internal_fb.o(.conststring), (152 bytes).
    Removing hal_internal_svs.o(.rev16_text), (4 bytes).
    Removing hal_internal_svs.o(.revsh_text), (4 bytes).
    Removing hal_internal_svs.o(i.hal_intl_svs_set_input_frate), (112 bytes).
    Removing hal_internal_svs.o(i.hal_intl_svs_set_sync_coef), (12 bytes).
    Removing drv_common.o(.rev16_text), (4 bytes).
    Removing drv_common.o(.revsh_text), (4 bytes).
    Removing drv_common.o(i.drv_common_disable_systick), (20 bytes).
    Removing drv_common.o(i.drv_common_enable_systick), (88 bytes).
    Removing drv_common.o(i.drv_common_get_tick), (12 bytes).
    Removing drv_common.o(i.drv_common_idle_mode), (40 bytes).
    Removing drv_common.o(i.drv_common_systick_register_cb), (12 bytes).
    Removing drv_crgu.o(.rev16_text), (4 bytes).
    Removing drv_crgu.o(.revsh_text), (4 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_all_reset_flags), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_clear_reset_flag), (20 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_all_reset_flag), (12 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_reset_flag), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_get_system_clk), (104 bytes).
    Removing drv_crgu.o(i.drv_crgu_reset_chip), (24 bytes).
    Removing drv_crgu.o(i.drv_crgu_set_clock_src), (16 bytes).
    Removing drv_dma.o(.rev16_text), (4 bytes).
    Removing drv_dma.o(.revsh_text), (4 bytes).
    Removing drv_dma.o(i.drv_dma_apply_handle), (304 bytes).
    Removing drv_dma.o(i.drv_dma_deinit), (52 bytes).
    Removing drv_dma.o(i.drv_dma_disable), (20 bytes).
    Removing drv_dma.o(i.drv_dma_disable_int), (40 bytes).
    Removing drv_dma.o(i.drv_dma_enable), (36 bytes).
    Removing drv_dma.o(i.drv_dma_enable_int), (68 bytes).
    Removing drv_dma.o(i.drv_dma_get_remaining_trans_num), (20 bytes).
    Removing drv_dma.o(i.drv_dma_get_status), (20 bytes).
    Removing drv_dma.o(i.drv_dma_init), (22 bytes).
    Removing drv_dma.o(i.drv_dma_int_list_delete), (88 bytes).
    Removing drv_dma.o(i.drv_dma_int_list_inset), (48 bytes).
    Removing drv_dma.o(i.drv_dma_register_callback), (4 bytes).
    Removing drv_dma.o(i.drv_dma_reset), (36 bytes).
    Removing drv_dma.o(i.drv_dma_set_bitwide), (56 bytes).
    Removing drv_dma.o(i.drv_dma_set_burst), (20 bytes).
    Removing drv_dma.o(i.drv_dma_set_circle_mode), (40 bytes).
    Removing drv_dma.o(i.drv_dma_set_dir), (40 bytes).
    Removing drv_dma.o(i.drv_dma_set_increment), (72 bytes).
    Removing drv_dma.o(i.drv_dma_set_mem_trans_info), (40 bytes).
    Removing drv_dma.o(i.drv_dma_set_mem_trans_offset), (24 bytes).
    Removing drv_dma.o(i.drv_dma_set_per_address), (20 bytes).
    Removing drv_dma.o(i.drv_dma_set_priority), (32 bytes).
    Removing drv_dma.o(i.drv_dma_set_tran_int_cnt), (28 bytes).
    Removing drv_dma.o(i.drv_dma_update_handle_setting), (148 bytes).
    Removing drv_dma.o(i.drv_dma_update_req_by_default), (40 bytes).
    Removing drv_dma.o(.constdata), (136 bytes).
    Removing drv_dsc_dec.o(.rev16_text), (4 bytes).
    Removing drv_dsc_dec.o(.revsh_text), (4 bytes).
    Removing drv_gpio.o(.rev16_text), (4 bytes).
    Removing drv_gpio.o(.revsh_text), (4 bytes).
    Removing drv_gpio.o(i.drv_gpio_get_attribute), (16 bytes).
    Removing drv_gpio.o(i.drv_gpio_get_input_data), (24 bytes).
    Removing drv_gpio.o(i.drv_gpio_set_attribute), (28 bytes).
    Removing drv_pwr.o(.rev16_text), (4 bytes).
    Removing drv_pwr.o(.revsh_text), (4 bytes).
    Removing drv_pwr.o(i.drv_pwr_10bit_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_analog_pwm_en), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_charge_pump_en), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_close_iov18_tp18), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_dsc_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_elvcc_pwm_en), (124 bytes).
    Removing drv_pwr.o(i.drv_pwr_enter_sleep_mode), (152 bytes).
    Removing drv_pwr.o(i.drv_pwr_exit_sleep_mode_ex), (40 bytes).
    Removing drv_pwr.o(i.drv_pwr_fb_pd), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_get_wakeflag), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_get_write_lock_st), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_hf_frm_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_10M_clock), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_mode_clock_sel), (60 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_mode_sel), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_hv_ldo_voltage_set), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo11d_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo13s_en), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo13s_set), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo15_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo18s_en), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_ldo18s_set), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_ltpo_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_osc32k_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_osc80m_trim), (36 bytes).
    Removing drv_pwr.o(i.drv_pwr_p3k_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_por_mode_flag), (32 bytes).
    Removing drv_pwr.o(i.drv_pwr_power_in), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_power_ready_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_power_sel), (44 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwm_output_pwm_led), (56 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_driver_current_Big_step), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_driver_current_small_step), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_electric_current), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_pwmled_open_drain), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_ram_pd_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_read_boot_chipst), (12 bytes).
    Removing drv_pwr.o(i.drv_pwr_read_chipcfg), (12 bytes).
    Removing drv_pwr.o(i.drv_pwr_rgbr_state_get), (16 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_ap_rst_mode), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_ldo11_mode), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_ldo15_mode), (48 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_pvd), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_pvd_mode), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_set_system_clk), (32 bytes).
    Removing drv_pwr.o(i.drv_pwr_sw_tp18_en), (52 bytes).
    Removing drv_pwr.o(i.drv_pwr_wakeflag_get), (16 bytes).
    Removing drv_spi_master.o(.rev16_text), (4 bytes).
    Removing drv_spi_master.o(.revsh_text), (4 bytes).
    Removing drv_spi_master.o(i.drv_spim_enable_int), (40 bytes).
    Removing drv_spi_master.o(i.drv_spim_init), (100 bytes).
    Removing drv_spi_master.o(i.drv_spim_read), (104 bytes).
    Removing drv_spi_master.o(i.drv_spim_write), (64 bytes).
    Removing drv_swire.o(.rev16_text), (4 bytes).
    Removing drv_swire.o(.revsh_text), (4 bytes).
    Removing drv_sys_cfg.o(.rev16_text), (4 bytes).
    Removing drv_sys_cfg.o(.revsh_text), (4 bytes).
    Removing drv_sys_cfg.o(i.drv_sys_cfg_sel_dma_req), (128 bytes).
    Removing drv_timer.o(.rev16_text), (4 bytes).
    Removing drv_timer.o(.revsh_text), (4 bytes).
    Removing drv_timer.o(i.drv_timer_get_status), (38 bytes).
    Removing drv_wdg.o(.rev16_text), (4 bytes).
    Removing drv_wdg.o(.revsh_text), (4 bytes).
    Removing drv_wdg.o(i.drv_wdg_enable), (32 bytes).
    Removing drv_wdg.o(i.drv_wdg_load_match), (12 bytes).
    Removing drv_wdg.o(i.drv_wdg_register_callback), (12 bytes).
    Removing drv_wdg.o(i.drv_wdg_sel_mode), (28 bytes).
    Removing drv_wdg.o(i.drv_wdg_set_repeat), (12 bytes).
    Removing drv_crc.o(.rev16_text), (4 bytes).
    Removing drv_crc.o(.revsh_text), (4 bytes).
    Removing drv_crc.o(i.drv_crc_dma_disable), (16 bytes).
    Removing drv_crc.o(i.drv_crc_dma_enable), (16 bytes).
    Removing drv_crc.o(i.drv_crc_get_data_register), (12 bytes).
    Removing drv_crc.o(i.drv_crc_get_fxor_register), (16 bytes).
    Removing drv_crc.o(i.drv_crc_get_idr_counter), (12 bytes).
    Removing drv_crc.o(i.drv_crc_get_initial_seed_register), (12 bytes).
    Removing drv_crc.o(i.drv_crc_get_polynomial_register), (12 bytes).
    Removing drv_crc.o(i.drv_crc_get_rev_in_register), (16 bytes).
    Removing drv_crc.o(i.drv_crc_get_rev_out_register), (16 bytes).
    Removing drv_crc.o(i.drv_crc_get_tcrc_register), (16 bytes).
    Removing drv_crc.o(i.drv_crc_reset), (16 bytes).
    Removing drv_crc.o(i.drv_crc_set_fxor_register), (28 bytes).
    Removing drv_crc.o(i.drv_crc_set_initial_seed_register), (12 bytes).
    Removing drv_crc.o(i.drv_crc_set_polynomial_register), (12 bytes).
    Removing drv_crc.o(i.drv_crc_set_rev_in_register), (24 bytes).
    Removing drv_crc.o(i.drv_crc_set_rev_out_register), (28 bytes).
    Removing drv_crc.o(i.drv_crc_set_tcrc_register), (28 bytes).
    Removing drv_crc.o(i.drv_crc_write_data_register), (28 bytes).
    Removing drv_i2c.o(.rev16_text), (4 bytes).
    Removing drv_i2c.o(.revsh_text), (4 bytes).
    Removing drv_i2c.o(i.__NVIC_DisableIRQ), (32 bytes).
    Removing drv_i2c.o(i.drv_i2c_NVIC_enable), (52 bytes).
    Removing drv_i2c.o(i.drv_i2c_clear_intr_status), (72 bytes).
    Removing drv_i2c.o(i.drv_i2c_clock_enable), (52 bytes).
    Removing drv_i2c.o(i.drv_i2c_disable_dma_req), (24 bytes).
    Removing drv_i2c.o(i.drv_i2c_disable_intr), (20 bytes).
    Removing drv_i2c.o(i.drv_i2c_enable), (36 bytes).
    Removing drv_i2c.o(i.drv_i2c_enable_dma_req), (24 bytes).
    Removing drv_i2c.o(i.drv_i2c_enable_intr), (56 bytes).
    Removing drv_i2c.o(i.drv_i2c_flush), (24 bytes).
    Removing drv_i2c.o(i.drv_i2c_get_fifo_status), (36 bytes).
    Removing drv_i2c.o(i.drv_i2c_get_intr_status), (16 bytes).
    Removing drv_i2c.o(i.drv_i2c_get_rx_count), (20 bytes).
    Removing drv_i2c.o(i.drv_i2c_get_tx_abrtsource), (20 bytes).
    Removing drv_i2c.o(i.drv_i2c_read_data), (44 bytes).
    Removing drv_i2c.o(i.drv_i2c_set_callback), (16 bytes).
    Removing drv_i2c.o(i.drv_i2c_set_fifo_threshold), (32 bytes).
    Removing drv_i2c.o(i.drv_i2c_set_sys_mask), (48 bytes).
    Removing drv_i2c.o(i.drv_i2c_write_data), (40 bytes).
    Removing drv_i2c.o(i.drv_i2cm_cal_scl_cnt), (40 bytes).
    Removing drv_i2c.o(i.drv_i2cm_init), (156 bytes).
    Removing drv_i2c.o(i.drv_i2cm_multi_params_read_data), (132 bytes).
    Removing drv_i2c.o(i.drv_i2cm_read_data), (140 bytes).
    Removing drv_i2c.o(i.drv_i2cm_set_baud_rate), (76 bytes).
    Removing drv_i2c.o(i.drv_i2cm_set_slave_addr), (52 bytes).
    Removing drv_i2c.o(i.drv_i2cm_write_data), (76 bytes).
    Removing drv_i2c.o(i.drv_i2cm_write_read_cmd), (60 bytes).
    Removing drv_i2c.o(i.drv_i2cs_init), (72 bytes).
    Removing drv_i2c.o(i.drv_i2cs_own_addr), (16 bytes).
    Removing drv_per_common.o(.rev16_text), (4 bytes).
    Removing drv_per_common.o(.revsh_text), (4 bytes).
    Removing drv_per_common.o(i.drv_per_get_system_clk), (8 bytes).
    Removing drv_per_common.o(i.drv_per_reset_module), (14 bytes).
    Removing drv_per_common.o(i.drv_per_set_clock), (14 bytes).
    Removing dcs_packet_fifo.o(.rev16_text), (4 bytes).
    Removing dcs_packet_fifo.o(.revsh_text), (4 bytes).
    Removing dcs_packet_fifo.o(i.dcs_packet_get_fifo_size), (16 bytes).
    Removing drv_se.o(.rev16_text), (4 bytes).
    Removing drv_se.o(.revsh_text), (4 bytes).
    Removing drv_dsi_rx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_rx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_force_video_crtl), (28 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_lpdt_fifo_status), (16 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_max_ret_size), (12 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_phy_stopstate), (68 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_get_version), (12 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_pg_cfg), (24 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_drv_log_level), (12 bytes).
    Removing drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_pg_cfg), (48 bytes).
    Removing drv_dsi_tx.o(.rev16_text), (4 bytes).
    Removing drv_dsi_tx.o(.revsh_text), (4 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_command_get_payload), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_force_interrupt), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_get_phy_status), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_forcepll), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_start), (24 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_pll_lock), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ulpsactivenot), (68 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_trigger), (92 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_enter), (296 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_phy_ulps_exit), (228 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_sdf_3d), (32 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_bta), (28 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_set_vpg), (100 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_version), (12 bytes).
    Removing drv_dsi_tx.o(i.drv_dsi_tx_vid_shadow), (20 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_clear), (16 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_lock), (32 bytes).
    Removing drv_dsi_tx.o(i.drv_tx_phy_test_read), (16 bytes).
    Removing drv_lcdc.o(.rev16_text), (4 bytes).
    Removing drv_lcdc.o(.revsh_text), (4 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_clear_irq), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_dpisignal_output_ctrl), (44 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_fixed_frame_output), (56 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_dpbuf_num), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_dpi_status), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_frame_clk_count), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_int_en_status), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_int_status), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_line_status), (12 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_get_rgb2pen_subpixel), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_part_display_config), (52 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_pixel_value_config), (32 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_rd_st_line_config), (28 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_software_reset), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_update_shadow_reg), (16 bytes).
    Removing drv_lcdc.o(i.drv_lcdc_vid_sw_start), (56 bytes).
    Removing drv_memc.o(.rev16_text), (4 bytes).
    Removing drv_memc.o(.revsh_text), (4 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_frm_time), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_db_int_frame), (36 bytes).
    Removing drv_memc.o(i.drv_memc_set_double_buffer_reverse), (24 bytes).
    Removing drv_memc.o(i.drv_memc_set_fb_pri), (44 bytes).
    Removing drv_memc.o(i.drv_memc_set_fb_remaining_line_trigger), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_inten), (28 bytes).
    Removing drv_memc.o(i.drv_memc_set_read_trigger_line), (24 bytes).
    Removing drv_memc.o(i.drv_memc_set_te_ind), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_tear_hwclr), (24 bytes).
    Removing drv_memc.o(i.drv_memc_set_vidc_fb_arb), (20 bytes).
    Removing drv_memc.o(i.drv_memc_set_write_trigger_line), (24 bytes).
    Removing drv_rxbr.o(.rev16_text), (4 bytes).
    Removing drv_rxbr.o(.revsh_text), (4 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_clr_swp_cnt), (16 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_dsc_flush), (24 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_col_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_cur_hline_rcv_cnt), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_frame_data_interval), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_hline_dcat), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_ipi_vsync_interval), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_page_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_pix_fmt), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_get_swpxl_cnt), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_hline_rcv0_cfg), (20 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_register_irq0_callback), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_ack_pkt_header), (24 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_ack_pkt_md), (28 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_cmd_filter), (320 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_col_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_compress), (32 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_data_catch_hline), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_page_addr), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_swpxl_data), (12 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_set_tmpdith_bp), (28 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_soft_reset), (32 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_sw_reset), (164 bytes).
    Removing drv_rxbr.o(i.drv_rxbr_swpxl_clr), (32 bytes).
    Removing drv_vidc.o(.rev16_text), (4 bytes).
    Removing drv_vidc.o(.revsh_text), (4 bytes).
    Removing drv_vidc.o(i.drv_vidc_clear_status0), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_cap_pixel), (28 bytes).
    Removing drv_vidc.o(i.drv_vidc_debug_signal_frame), (36 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status0), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status1), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_get_status2), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_dsc_thresh), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_frmst_latency), (20 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_inff_thresh), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_irq_line), (24 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_module_enable), (28 bytes).
    Removing drv_vidc.o(i.drv_vidc_set_outff_thresh), (12 bytes).
    Removing drv_vidc.o(i.drv_vidc_update_src_format), (20 bytes).
    Removing drv_uart.o(.rev16_text), (4 bytes).
    Removing drv_uart.o(.revsh_text), (4 bytes).
    Removing drv_uart.o(i.drv_uart_deinit), (60 bytes).
    Removing drv_uart.o(i.drv_uart_get_def_cfg), (72 bytes).
    Removing drv_uart.o(i.drv_uart_recv_blocking), (48 bytes).
    Removing drv_uart.o(i.drv_uart_recv_none_blocking), (60 bytes).
    Removing drv_uart.o(i.drv_uart_send_none_blocking), (60 bytes).
    Removing drv_efuse.o(.rev16_text), (4 bytes).
    Removing drv_efuse.o(.revsh_text), (4 bytes).
    Removing drv_efuse.o(i.drv_efuse_crc_cal), (128 bytes).
    Removing drv_efuse.o(i.drv_efuse_get_default_config), (26 bytes).
    Removing drv_efuse.o(i.drv_efuse_int_disable), (12 bytes).
    Removing drv_efuse.o(i.drv_efuse_write), (56 bytes).
    Removing drv_efuse.o(i.drv_efuse_write_read_req_clear), (22 bytes).
    Removing drv_efuse.o(i.drv_efuse_write_req), (22 bytes).
    Removing drv_phy_common.o(.rev16_text), (4 bytes).
    Removing drv_phy_common.o(.revsh_text), (4 bytes).

561 unused section(s) (total 30473 bytes) removed from the image.

==============================================================================

Image Symbol Table

    Local Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    ../clib/../cmprslib/zerorunl2.c          0x00000000   Number         0  __dczerorl2.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uldiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  idiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uidiv.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry5.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry2.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7b.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llushr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llshl.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llsshr.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf6.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf5.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf4.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf2.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf1.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf0.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfb.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfa.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf3.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf8.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf7.o ABSOLUTE
    ../clib/microlib/printf/stubs.s          0x00000000   Number         0  stubs.o ABSOLUTE
    ../clib/microlib/stdio/streams.c         0x00000000   Number         0  stdout.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpyb.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpya.o ABSOLUTE
    ../clib/microlib/string/memset.c         0x00000000   Number         0  memseta.o ABSOLUTE
    ../clib/microlib/string/strlen.c         0x00000000   Number         0  strlen.o ABSOLUTE
    ../clib/microlib/stubs.s                 0x00000000   Number         0  iusefp.o ABSOLUTE
    ../fplib/microlib/d2f.c                  0x00000000   Number         0  d2f.o ABSOLUTE
    ../fplib/microlib/f2d.c                  0x00000000   Number         0  f2d.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  fadd.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  dadd.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  fdiv.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  ddiv.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  fepilogue.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  depilogue.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  ffixui.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixui.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixul.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  dfltui.o ABSOLUTE
    ../fplib/microlib/fpflt.c                0x00000000   Number         0  ffltui.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  fmul.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  dmul.o ABSOLUTE
    ../fplib/microlib/fpscalb.c              0x00000000   Number         0  fscalb.o ABSOLUTE
    ../mathlib/ceil.c                        0x00000000   Number         0  ceil.o ABSOLUTE
    ..\..\..\src\common\tau_delay.c          0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\..\..\src\common\tau_log.c            0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_crc.c 0x00000000   Number         0  drv_crc.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_i2c.c 0x00000000   Number         0  drv_i2c.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_per_common.c 0x00000000   Number         0  drv_per_common.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_spi_master.c 0x00000000   Number         0  drv_spi_master.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\drv\drv_wdg.c 0x00000000   Number         0  drv_wdg.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_crc.c 0x00000000   Number         0  hal_crc.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_i2c_slave.c 0x00000000   Number         0  hal_i2c_slave.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_pwr.c 0x00000000   Number         0  hal_pwr.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_spi_master.c 0x00000000   Number         0  hal_spi_master.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_swire.c 0x00000000   Number         0  hal_swire.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_timer.c 0x00000000   Number         0  hal_timer.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\hal_wdg.c 0x00000000   Number         0  hal_wdg.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\dcs_packet_fifo.c 0x00000000   Number         0  dcs_packet_fifo.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_dcs.c 0x00000000   Number         0  hal_internal_dcs.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_fb.c 0x00000000   Number         0  hal_internal_fb.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_svs.c 0x00000000   Number         0  hal_internal_svs.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\hal\internal\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\..\..\src\driver\cuckoo\src\drv_se.c  0x00000000   Number         0  drv_se.o ABSOLUTE
    ..\..\src\app\S8\app_tp_for_custom_s8.c  0x00000000   Number         0  app_tp_for_custom_s8.o ABSOLUTE
    ..\..\src\app\S8\s8_demo.c               0x00000000   Number         0  s8_demo.o ABSOLUTE
    ..\..\src\app\main.c                     0x00000000   Number         0  main.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_crc.c 0x00000000   Number         0  demo_hal_crc.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_dsi_rx.c 0x00000000   Number         0  demo_hal_dsi_rx.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_dsi_tx.c 0x00000000   Number         0  demo_hal_dsi_tx.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_flash.c 0x00000000   Number         0  demo_hal_flash.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_gpio.c 0x00000000   Number         0  demo_hal_gpio.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_i2c.c 0x00000000   Number         0  demo_hal_i2c.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_pwm.c 0x00000000   Number         0  demo_hal_pwm.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_pwr.c 0x00000000   Number         0  demo_hal_pwr.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_spi.c 0x00000000   Number         0  demo_hal_spi.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_swire.c 0x00000000   Number         0  demo_hal_swire.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_uart.c 0x00000000   Number         0  demo_hal_uart.o ABSOLUTE
    ..\..\src\app\module_demo\demo_hal_wdg.c 0x00000000   Number         0  demo_hal_wdg.o ABSOLUTE
    ..\..\src\app\module_demo\module_demo_main.c 0x00000000   Number         0  module_demo_main.o ABSOLUTE
    ..\..\src\app\touch\app_tp_transfer.c    0x00000000   Number         0  app_tp_transfer.o ABSOLUTE
    ..\..\src\board\board.c                  0x00000000   Number         0  board.o ABSOLUTE
    ..\..\src\board\startup\startup_ARMCM0.s 0x00000000   Number         0  startup_armcm0.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_delay.c     0x00000000   Number         0  tau_delay.o ABSOLUTE
    ..\\..\\..\\src\\common\\tau_log.c       0x00000000   Number         0  tau_log.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_common.c 0x00000000   Number         0  drv_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_crc.c 0x00000000   Number         0  drv_crc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_crgu.c 0x00000000   Number         0  drv_crgu.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dma.c 0x00000000   Number         0  drv_dma.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dsc_dec.c 0x00000000   Number         0  drv_dsc_dec.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dsi_rx.c 0x00000000   Number         0  drv_dsi_rx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_dsi_tx.c 0x00000000   Number         0  drv_dsi_tx.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_efuse.c 0x00000000   Number         0  drv_efuse.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_gpio.c 0x00000000   Number         0  drv_gpio.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_i2c.c 0x00000000   Number         0  drv_i2c.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_lcdc.c 0x00000000   Number         0  drv_lcdc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_memc.c 0x00000000   Number         0  drv_memc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_per_common.c 0x00000000   Number         0  drv_per_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_phy_common.c 0x00000000   Number         0  drv_phy_common.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_pwr.c 0x00000000   Number         0  drv_pwr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_rxbr.c 0x00000000   Number         0  drv_rxbr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_spi_master.c 0x00000000   Number         0  drv_spi_master.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_swire.c 0x00000000   Number         0  drv_swire.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_sys_cfg.c 0x00000000   Number         0  drv_sys_cfg.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_timer.c 0x00000000   Number         0  drv_timer.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_uart.c 0x00000000   Number         0  drv_uart.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_vidc.c 0x00000000   Number         0  drv_vidc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\drv\\drv_wdg.c 0x00000000   Number         0  drv_wdg.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_crc.c 0x00000000   Number         0  hal_crc.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_dsi_rx_ctrl.c 0x00000000   Number         0  hal_dsi_rx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_dsi_tx_ctrl.c 0x00000000   Number         0  hal_dsi_tx_ctrl.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_gpio.c 0x00000000   Number         0  hal_gpio.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_i2c_slave.c 0x00000000   Number         0  hal_i2c_slave.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_pwr.c 0x00000000   Number         0  hal_pwr.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_spi_master.c 0x00000000   Number         0  hal_spi_master.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_swire.c 0x00000000   Number         0  hal_swire.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_system.c 0x00000000   Number         0  hal_system.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_timer.c 0x00000000   Number         0  hal_timer.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_uart.c 0x00000000   Number         0  hal_uart.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\hal_wdg.c 0x00000000   Number         0  hal_wdg.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\dcs_packet_fifo.c 0x00000000   Number         0  dcs_packet_fifo.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_dcs.c 0x00000000   Number         0  hal_internal_dcs.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_fb.c 0x00000000   Number         0  hal_internal_fb.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_svs.c 0x00000000   Number         0  hal_internal_svs.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\hal\\internal\\hal_internal_vsync.c 0x00000000   Number         0  hal_internal_vsync.o ABSOLUTE
    ..\\..\\..\\src\\driver\\cuckoo\\src\\drv_se.c 0x00000000   Number         0  drv_se.o ABSOLUTE
    ..\\..\\src\\app\\S8\\app_tp_for_custom_s8.c 0x00000000   Number         0  app_tp_for_custom_s8.o ABSOLUTE
    ..\\..\\src\\app\\S8\\s8_demo.c          0x00000000   Number         0  s8_demo.o ABSOLUTE
    ..\\..\\src\\app\\main.c                 0x00000000   Number         0  main.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_crc.c 0x00000000   Number         0  demo_hal_crc.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_dsi_rx.c 0x00000000   Number         0  demo_hal_dsi_rx.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_dsi_tx.c 0x00000000   Number         0  demo_hal_dsi_tx.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_flash.c 0x00000000   Number         0  demo_hal_flash.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_gpio.c 0x00000000   Number         0  demo_hal_gpio.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_i2c.c 0x00000000   Number         0  demo_hal_i2c.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_pwm.c 0x00000000   Number         0  demo_hal_pwm.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_pwr.c 0x00000000   Number         0  demo_hal_pwr.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_spi.c 0x00000000   Number         0  demo_hal_spi.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_swire.c 0x00000000   Number         0  demo_hal_swire.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_uart.c 0x00000000   Number         0  demo_hal_uart.o ABSOLUTE
    ..\\..\\src\\app\\module_demo\\demo_hal_wdg.c 0x00000000   Number         0  demo_hal_wdg.o ABSOLUTE
    ..\\..\\src\\app\\touch\\app_tp_transfer.c 0x00000000   Number         0  app_tp_transfer.o ABSOLUTE
    ..\\..\\src\\board\\board.c              0x00000000   Number         0  board.o ABSOLUTE
    cdrcmple.s                               0x00000000   Number         0  cdrcmple.o ABSOLUTE
    cfcmple.s                                0x00000000   Number         0  cfcmple.o ABSOLUTE
    cfrcmple.s                               0x00000000   Number         0  cfrcmple.o ABSOLUTE
    dc.s                                     0x00000000   Number         0  dc.o ABSOLUTE
    handlers.s                               0x00000000   Number         0  handlers.o ABSOLUTE
    init.s                                   0x00000000   Number         0  init.o ABSOLUTE
    RESET                                    0x00010000   Section      192  startup_armcm0.o(RESET)
    .ARM.Collect$$$$00000000                 0x000100c0   Section        0  entry.o(.ARM.Collect$$$$00000000)
    .ARM.Collect$$$$00000001                 0x000100c0   Section        4  entry2.o(.ARM.Collect$$$$00000001)
    .ARM.Collect$$$$00000004                 0x000100c4   Section        4  entry5.o(.ARM.Collect$$$$00000004)
    .ARM.Collect$$$$00000008                 0x000100c8   Section        0  entry7b.o(.ARM.Collect$$$$00000008)
    .ARM.Collect$$$$0000000A                 0x000100c8   Section        0  entry8b.o(.ARM.Collect$$$$0000000A)
    .ARM.Collect$$$$0000000B                 0x000100c8   Section        8  entry9a.o(.ARM.Collect$$$$0000000B)
    .ARM.Collect$$$$0000000D                 0x000100d0   Section        0  entry10a.o(.ARM.Collect$$$$0000000D)
    .ARM.Collect$$$$0000000F                 0x000100d0   Section        0  entry11a.o(.ARM.Collect$$$$0000000F)
    .ARM.Collect$$$$00002712                 0x000100d0   Section        4  entry2.o(.ARM.Collect$$$$00002712)
    __lit__00000000                          0x000100d0   Data           4  entry2.o(.ARM.Collect$$$$00002712)
    .text                                    0x000100d4   Section      120  startup_armcm0.o(.text)
    .text                                    0x0001014c   Section        0  uidiv.o(.text)
    .text                                    0x00010178   Section        0  idiv.o(.text)
    .text                                    0x000101a0   Section        0  memcpya.o(.text)
    .text                                    0x000101c4   Section        0  memseta.o(.text)
    .text                                    0x000101e8   Section        0  strlen.o(.text)
    .text                                    0x000101f6   Section        0  fadd.o(.text)
    .text                                    0x000102a8   Section        0  fmul.o(.text)
    .text                                    0x00010322   Section        0  fdiv.o(.text)
    .text                                    0x0001039e   Section        0  fscalb.o(.text)
    .text                                    0x000103b8   Section        0  dadd.o(.text)
    .text                                    0x0001051c   Section        0  dmul.o(.text)
    .text                                    0x000105ec   Section        0  ddiv.o(.text)
    .text                                    0x000106dc   Section        0  ffltui.o(.text)
    .text                                    0x000106ec   Section        0  dfltui.o(.text)
    .text                                    0x00010708   Section        0  ffixui.o(.text)
    .text                                    0x00010730   Section        0  dfixui.o(.text)
    .text                                    0x0001076c   Section        0  f2d.o(.text)
    .text                                    0x00010794   Section        0  d2f.o(.text)
    .text                                    0x000107cc   Section       20  cfcmple.o(.text)
    .text                                    0x000107e0   Section       20  cfrcmple.o(.text)
    .text                                    0x000107f4   Section        0  uldiv.o(.text)
    .text                                    0x00010854   Section        0  llshl.o(.text)
    .text                                    0x00010874   Section        0  llushr.o(.text)
    .text                                    0x00010896   Section        0  llsshr.o(.text)
    .text                                    0x000108bc   Section        0  fepilogue.o(.text)
    .text                                    0x000108bc   Section        0  iusefp.o(.text)
    .text                                    0x0001093e   Section        0  depilogue.o(.text)
    .text                                    0x000109fc   Section        0  dfixul.o(.text)
    .text                                    0x00010a3c   Section       40  cdrcmple.o(.text)
    .text                                    0x00010a64   Section       36  init.o(.text)
    .text                                    0x00010a88   Section        0  __dczerorl2.o(.text)
    i.AP_NRESET_IRQn_Handler                 0x00010ae0   Section        0  drv_gpio.o(i.AP_NRESET_IRQn_Handler)
    i.DMA_IRQn_Handler                       0x00010afc   Section        0  drv_dma.o(i.DMA_IRQn_Handler)
    i.EXTI_INT0_IRQn_Handler                 0x00010b58   Section        0  drv_gpio.o(i.EXTI_INT0_IRQn_Handler)
    i.EXTI_INT1_IRQn_Handler                 0x00010b62   Section        0  drv_gpio.o(i.EXTI_INT1_IRQn_Handler)
    i.EXTI_INT2_IRQn_Handler                 0x00010b6c   Section        0  drv_gpio.o(i.EXTI_INT2_IRQn_Handler)
    i.EXTI_INT3_IRQn_Handler                 0x00010b76   Section        0  drv_gpio.o(i.EXTI_INT3_IRQn_Handler)
    i.EXTI_INT4_IRQn_Handler                 0x00010b80   Section        0  drv_gpio.o(i.EXTI_INT4_IRQn_Handler)
    i.EXTI_INT5_IRQn_Handler                 0x00010b8a   Section        0  drv_gpio.o(i.EXTI_INT5_IRQn_Handler)
    i.EXTI_INT6_IRQn_Handler                 0x00010b94   Section        0  drv_gpio.o(i.EXTI_INT6_IRQn_Handler)
    i.EXTI_INT7_IRQn_Handler                 0x00010b9e   Section        0  drv_gpio.o(i.EXTI_INT7_IRQn_Handler)
    i.HardFault_Handler                      0x00010ba8   Section        0  drv_common.o(i.HardFault_Handler)
    i.I2C0_IRQn_Handler                      0x00010bf0   Section        0  drv_i2c.o(i.I2C0_IRQn_Handler)
    i.I2C1_IRQn_Handler                      0x00010bfc   Section        0  drv_i2c.o(i.I2C1_IRQn_Handler)
    i.I2C2_IRQn_Handler                      0x00010c08   Section        0  drv_i2c.o(i.I2C2_IRQn_Handler)
    i.LCDC_IRQn_Handler                      0x00010c14   Section        0  hal_internal_vsync.o(i.LCDC_IRQn_Handler)
    i.MEMC_IRQn_Handler                      0x00010d14   Section        0  drv_memc.o(i.MEMC_IRQn_Handler)
    i.MIPI_TX_IRQn_Handler                   0x00010db0   Section        0  drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler)
    i.SPIM_IRQn_Handler                      0x00010e68   Section        0  hal_spi_master.o(i.SPIM_IRQn_Handler)
    i.SWIRE_IRQn_Handler                     0x00010eb0   Section        0  drv_swire.o(i.SWIRE_IRQn_Handler)
    i.SysTick_Handler                        0x00010ee0   Section        0  drv_common.o(i.SysTick_Handler)
    i.TIMER0_IRQn_Handler                    0x00010ef8   Section        0  drv_timer.o(i.TIMER0_IRQn_Handler)
    i.TIMER1_IRQn_Handler                    0x00010f02   Section        0  drv_timer.o(i.TIMER1_IRQn_Handler)
    i.TIMER2_IRQn_Handler                    0x00010f0c   Section        0  drv_timer.o(i.TIMER2_IRQn_Handler)
    i.TIMER3_IRQn_Handler                    0x00010f16   Section        0  drv_timer.o(i.TIMER3_IRQn_Handler)
    i.VIDC_IRQn_Handler                      0x00010f20   Section        0  drv_vidc.o(i.VIDC_IRQn_Handler)
    i.VPRE1_IRQn_Handler                     0x00010f3c   Section        0  drv_rxbr.o(i.VPRE1_IRQn_Handler)
    i.VPRE_IRQn_Handler                      0x00010f58   Section        0  hal_internal_dcs.o(i.VPRE_IRQn_Handler)
    i.WDG_IRQn_Handler                       0x00010fc4   Section        0  drv_wdg.o(i.WDG_IRQn_Handler)
    i.__scatterload_null                     0x00010ffc   Section        2  handlers.o(i.__scatterload_null)
    .ARM.__at_0x11000                        0x00011000   Section       28  drv_common.o(.ARM.__at_0x11000)
    .ARM.__at_0x1101C                        0x0001101c   Section       16  tau_log.o(.ARM.__at_0x1101C)
    .ARM.__at_0x1102C                        0x0001102c   Section       22  hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C)
    i.MIPI_RX_IRQn_Handler                   0x00011044   Section        0  drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler)
    i.UART_IRQn_Handler                      0x000113a8   Section        0  drv_uart.o(i.UART_IRQn_Handler)
    i.__0printf                              0x00011528   Section        0  printfa.o(i.__0printf)
    i.__0vsprintf                            0x00011548   Section        0  printfa.o(i.__0vsprintf)
    i.__ARM_clz                              0x0001156c   Section        0  depilogue.o(i.__ARM_clz)
    i.__ARM_common_switch8                   0x0001159a   Section        0  hal_dsi_rx_ctrl.o(i.__ARM_common_switch8)
    i.__NVIC_DisableIRQ                      0x000115b4   Section        0  drv_rxbr.o(i.__NVIC_DisableIRQ)
    __NVIC_DisableIRQ                        0x000115b5   Thumb Code    26  drv_rxbr.o(i.__NVIC_DisableIRQ)
    i.__NVIC_EnableIRQ                       0x000115d4   Section        0  drv_rxbr.o(i.__NVIC_EnableIRQ)
    __NVIC_EnableIRQ                         0x000115d5   Thumb Code    18  drv_rxbr.o(i.__NVIC_EnableIRQ)
    i.__scatterload_copy                     0x000115ec   Section       14  handlers.o(i.__scatterload_copy)
    i.__scatterload_zeroinit                 0x000115fa   Section       14  handlers.o(i.__scatterload_zeroinit)
    i._fp_digits                             0x00011608   Section        0  printfa.o(i._fp_digits)
    _fp_digits                               0x00011609   Thumb Code   344  printfa.o(i._fp_digits)
    i._printf_core                           0x0001177c   Section        0  printfa.o(i._printf_core)
    _printf_core                             0x0001177d   Thumb Code  1754  printfa.o(i._printf_core)
    i._printf_post_padding                   0x00011e68   Section        0  printfa.o(i._printf_post_padding)
    _printf_post_padding                     0x00011e69   Thumb Code    32  printfa.o(i._printf_post_padding)
    i._printf_pre_padding                    0x00011e88   Section        0  printfa.o(i._printf_pre_padding)
    _printf_pre_padding                      0x00011e89   Thumb Code    44  printfa.o(i._printf_pre_padding)
    i._sputc                                 0x00011eb4   Section        0  printfa.o(i._sputc)
    _sputc                                   0x00011eb5   Thumb Code    10  printfa.o(i._sputc)
    i.ap_dcs_set_backlight                   0x00011ec0   Section        0  s8_demo.o(i.ap_dcs_set_backlight)
    ap_dcs_set_backlight                     0x00011ec1   Thumb Code   158  s8_demo.o(i.ap_dcs_set_backlight)
    i.ap_dcs_set_display_off                 0x00011f70   Section        0  s8_demo.o(i.ap_dcs_set_display_off)
    ap_dcs_set_display_off                   0x00011f71   Thumb Code     6  s8_demo.o(i.ap_dcs_set_display_off)
    i.ap_dcs_set_display_on                  0x00011f78   Section        0  s8_demo.o(i.ap_dcs_set_display_on)
    ap_dcs_set_display_on                    0x00011f79   Thumb Code    28  s8_demo.o(i.ap_dcs_set_display_on)
    i.ap_dcs_set_enter_sleep_mode            0x00011fb4   Section        0  s8_demo.o(i.ap_dcs_set_enter_sleep_mode)
    ap_dcs_set_enter_sleep_mode              0x00011fb5   Thumb Code    74  s8_demo.o(i.ap_dcs_set_enter_sleep_mode)
    i.ap_dcs_set_exit_sleep_mode             0x00012004   Section        0  s8_demo.o(i.ap_dcs_set_exit_sleep_mode)
    ap_dcs_set_exit_sleep_mode               0x00012005   Thumb Code    50  s8_demo.o(i.ap_dcs_set_exit_sleep_mode)
    i.ap_rstn_pull_high_cb                   0x00012068   Section        0  s8_demo.o(i.ap_rstn_pull_high_cb)
    ap_rstn_pull_high_cb                     0x00012069   Thumb Code    38  s8_demo.o(i.ap_rstn_pull_high_cb)
    i.ap_set_framerate                       0x000120bc   Section        0  s8_demo.o(i.ap_set_framerate)
    ap_set_framerate                         0x000120bd   Thumb Code    76  s8_demo.o(i.ap_set_framerate)
    i.ap_update_pps_9E                       0x0001213c   Section        0  s8_demo.o(i.ap_update_pps_9E)
    ap_update_pps_9E                         0x0001213d   Thumb Code   122  s8_demo.o(i.ap_update_pps_9E)
    i.app_display_init                       0x000121c0   Section        0  s8_demo.o(i.app_display_init)
    i.app_gpio_init                          0x00012228   Section        0  s8_demo.o(i.app_gpio_init)
    i.app_init_panel                         0x00012248   Section        0  s8_demo.o(i.app_init_panel)
    app_init_panel                           0x00012249   Thumb Code    64  s8_demo.o(i.app_init_panel)
    i.app_mipi_rx_init                       0x00012290   Section        0  s8_demo.o(i.app_mipi_rx_init)
    app_mipi_rx_init                         0x00012291   Thumb Code   212  s8_demo.o(i.app_mipi_rx_init)
    i.app_mipi_tx_init                       0x00012378   Section        0  s8_demo.o(i.app_mipi_tx_init)
    app_mipi_tx_init                         0x00012379   Thumb Code   188  s8_demo.o(i.app_mipi_tx_init)
    i.app_mipi_tx_start                      0x00012438   Section        0  s8_demo.o(i.app_mipi_tx_start)
    app_mipi_tx_start                        0x00012439   Thumb Code    62  s8_demo.o(i.app_mipi_tx_start)
    i.app_set_dcs_hw_ack                     0x000124a4   Section        0  s8_demo.o(i.app_set_dcs_hw_ack)
    app_set_dcs_hw_ack                       0x000124a5   Thumb Code   134  s8_demo.o(i.app_set_dcs_hw_ack)
    i.app_system_process                     0x00012530   Section        0  s8_demo.o(i.app_system_process)
    app_system_process                       0x00012531   Thumb Code    62  s8_demo.o(i.app_system_process)
    i.app_system_resume                      0x0001257c   Section        0  s8_demo.o(i.app_system_resume)
    app_system_resume                        0x0001257d   Thumb Code    30  s8_demo.o(i.app_system_resume)
    i.app_system_suspend                     0x000125c4   Section        0  s8_demo.o(i.app_system_suspend)
    app_system_suspend                       0x000125c5   Thumb Code   166  s8_demo.o(i.app_system_suspend)
    i.app_tx_panel_reset                     0x000126e8   Section        0  s8_demo.o(i.app_tx_panel_reset)
    app_tx_panel_reset                       0x000126e9   Thumb Code    46  s8_demo.o(i.app_tx_panel_reset)
    i.board_Init                             0x00012718   Section        0  board.o(i.board_Init)
    i.ceil                                   0x00012730   Section        0  ceil.o(i.ceil)
    i.check_mipi_rx_tx_video_info            0x000127f8   Section        0  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    check_mipi_rx_tx_video_info              0x000127f9   Thumb Code    44  hal_internal_vsync.o(i.check_mipi_rx_tx_video_info)
    i.check_pkt_buf_rev                      0x00012824   Section        0  hal_internal_dcs.o(i.check_pkt_buf_rev)
    check_pkt_buf_rev                        0x00012825   Thumb Code    84  hal_internal_dcs.o(i.check_pkt_buf_rev)
    i.dcs_packet_fifo_alloc                  0x000128ac   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    i.dcs_packet_fifo_init                   0x00012904   Section        0  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    i.dcs_packet_free_fifo_header            0x0001291c   Section        0  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    i.dcs_packet_get_fifo_header             0x00012960   Section        0  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    i.delayMs                                0x00012984   Section        0  tau_delay.o(i.delayMs)
    i.delayUs                                0x0001299c   Section        0  tau_delay.o(i.delayUs)
    i.drv_common_system_init                 0x000129c8   Section        0  drv_common.o(i.drv_common_system_init)
    i.drv_crgu_enable_clock                  0x000129d0   Section        0  drv_crgu.o(i.drv_crgu_enable_clock)
    i.drv_crgu_get_rxbr_clk                  0x00012a0c   Section        0  drv_crgu.o(i.drv_crgu_get_rxbr_clk)
    i.drv_crgu_reset_modules                 0x00012a74   Section        0  drv_crgu.o(i.drv_crgu_reset_modules)
    i.drv_crgu_set_ahb_clk                   0x00012a84   Section        0  drv_crgu.o(i.drv_crgu_set_ahb_clk)
    i.drv_crgu_set_clock_div                 0x00012aac   Section        0  drv_crgu.o(i.drv_crgu_set_clock_div)
    i.drv_crgu_set_dpi_clk                   0x00012abc   Section        0  drv_crgu.o(i.drv_crgu_set_dpi_clk)
    i.drv_crgu_set_dsc_clk                   0x00012af8   Section        0  drv_crgu.o(i.drv_crgu_set_dsc_clk)
    i.drv_crgu_set_fb_clk                    0x00012b30   Section        0  drv_crgu.o(i.drv_crgu_set_fb_clk)
    i.drv_crgu_set_lcdc_clk                  0x00012b58   Section        0  drv_crgu.o(i.drv_crgu_set_lcdc_clk)
    i.drv_crgu_set_reset                     0x00012b80   Section        0  drv_crgu.o(i.drv_crgu_set_reset)
    i.drv_crgu_set_rxbr_clk                  0x00012b98   Section        0  drv_crgu.o(i.drv_crgu_set_rxbr_clk)
    i.drv_crgu_set_vidc_clk                  0x00012bc0   Section        0  drv_crgu.o(i.drv_crgu_set_vidc_clk)
    i.drv_dma_clear_status                   0x00012be8   Section        0  drv_dma.o(i.drv_dma_clear_status)
    i.drv_dma_get_int_source                 0x00012c00   Section        0  drv_dma.o(i.drv_dma_get_int_source)
    drv_dma_get_int_source                   0x00012c01   Thumb Code    16  drv_dma.o(i.drv_dma_get_int_source)
    i.drv_dsc_dec_disable                    0x00012c14   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    i.drv_dsc_dec_enable                     0x00012c30   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    i.drv_dsc_dec_get_nslc                   0x00012c68   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    i.drv_dsc_dec_set_irqen                  0x00012c88   Section        0  drv_dsc_dec.o(i.drv_dsc_dec_set_irqen)
    i.drv_dsi_rx_calc_ipi_tx_delay           0x00012ca4   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    i.drv_dsi_rx_enable_irq                  0x00012db0   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    i.drv_dsi_rx_get_color_bpp               0x00012df0   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    drv_dsi_rx_get_color_bpp                 0x00012df1   Thumb Code    62  drv_dsi_rx.o(i.drv_dsi_rx_get_color_bpp)
    i.drv_dsi_rx_get_color_pcc               0x00012e40   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    drv_dsi_rx_get_color_pcc                 0x00012e41   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_get_color_pcc)
    i.drv_dsi_rx_get_compression_en          0x00012e5c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    i.drv_dsi_rx_get_ddi_crc_en              0x00012e6c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_get_ddi_crc_en)
    i.drv_dsi_rx_power_up                    0x00012e7c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    i.drv_dsi_rx_set_check_crc               0x00012e94   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc)
    i.drv_dsi_rx_set_ctrl_cfg                0x00012eb0   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    i.drv_dsi_rx_set_ddi_cfg                 0x00012ed4   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    i.drv_dsi_rx_set_ddi_crc_en              0x00012ee4   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_crc_en)
    i.drv_dsi_rx_set_inten                   0x00012f00   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    i.drv_dsi_rx_set_ipi_cfg                 0x00012f0c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    i.drv_dsi_rx_set_ipi_ycbcr_frmt          0x00012f1c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_ycbcr_frmt)
    i.drv_dsi_rx_set_lane_swap               0x00012f38   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    i.drv_dsi_rx_set_resp_cnt                0x00012f4c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    i.drv_dsi_rx_set_tear_resp_en            0x00012f70   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_tear_resp_en)
    i.drv_dsi_rx_set_up_phy                  0x00012f8c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    i.drv_dsi_rx_shut_down                   0x0001308c   Section        0  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    i.drv_dsi_tx_command_header              0x000130a4   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    i.drv_dsi_tx_command_mode_cfg            0x000130bc   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    i.drv_dsi_tx_command_put_payload         0x00013114   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    i.drv_dsi_tx_config_eotp                 0x00013120   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    i.drv_dsi_tx_config_int                  0x00013140   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    i.drv_dsi_tx_dpi_lpcmd_time              0x0001314c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    i.drv_dsi_tx_dpi_mode                    0x0001315c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    i.drv_dsi_tx_dpi_polarity                0x0001316c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    i.drv_dsi_tx_edpi_cmd_size               0x00013190   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    i.drv_dsi_tx_get_cmd_status              0x0001319c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    i.drv_dsi_tx_mode                        0x000131a8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    i.drv_dsi_tx_phy_clock_lane_auto_lp      0x000131b4   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    i.drv_dsi_tx_phy_clock_lane_req_hs       0x000131d0   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    i.drv_dsi_tx_phy_lane_mode               0x000131f0   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    i.drv_dsi_tx_phy_status_ready            0x00013200   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    i.drv_dsi_tx_phy_status_stopstate        0x00013268   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    i.drv_dsi_tx_phy_test_setup              0x000132ac   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    i.drv_dsi_tx_phy_time_cfg                0x000133fc   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    i.drv_dsi_tx_powerup                     0x0001341c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    i.drv_dsi_tx_response_mode               0x00013428   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    i.drv_dsi_tx_set_bta_ack                 0x0001344c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    i.drv_dsi_tx_set_esc_div                 0x00013468   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    i.drv_dsi_tx_set_int                     0x0001347c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    i.drv_dsi_tx_set_time_out_div            0x000134bc   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    i.drv_dsi_tx_set_video_chunk             0x000134d4   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    i.drv_dsi_tx_set_video_timing            0x000134e8   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    i.drv_dsi_tx_shutdown                    0x0001350c   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    i.drv_dsi_tx_timeout_cfg                 0x00013518   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    i.drv_dsi_tx_video_mode_cfg              0x00013544   Section        0  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    i.drv_efuse_enter_inactive               0x0001362c   Section        0  drv_efuse.o(i.drv_efuse_enter_inactive)
    i.drv_efuse_int_enable                   0x00013662   Section        0  drv_efuse.o(i.drv_efuse_int_enable)
    i.drv_efuse_read                         0x0001366e   Section        0  drv_efuse.o(i.drv_efuse_read)
    i.drv_efuse_read_req                     0x000136a8   Section        0  drv_efuse.o(i.drv_efuse_read_req)
    i.drv_gpio_handle_int                    0x000136c0   Section        0  drv_gpio.o(i.drv_gpio_handle_int)
    drv_gpio_handle_int                      0x000136c1   Thumb Code    30  drv_gpio.o(i.drv_gpio_handle_int)
    i.drv_gpio_register_ap_reset_callback    0x000136e4   Section        0  drv_gpio.o(i.drv_gpio_register_ap_reset_callback)
    i.drv_gpio_register_callback             0x000136f0   Section        0  drv_gpio.o(i.drv_gpio_register_callback)
    i.drv_gpio_set_int                       0x00013704   Section        0  drv_gpio.o(i.drv_gpio_set_int)
    i.drv_gpio_set_ioe                       0x00013748   Section        0  drv_gpio.o(i.drv_gpio_set_ioe)
    i.drv_gpio_set_mode                      0x00013768   Section        0  drv_gpio.o(i.drv_gpio_set_mode)
    i.drv_gpio_set_output_data               0x0001377c   Section        0  hal_gpio.o(i.drv_gpio_set_output_data)
    drv_gpio_set_output_data                 0x0001377d   Thumb Code    26  hal_gpio.o(i.drv_gpio_set_output_data)
    i.drv_lcdc_bcsa_config                   0x0001379c   Section        0  drv_lcdc.o(i.drv_lcdc_bcsa_config)
    i.drv_lcdc_cfg_int_frame                 0x000137c4   Section        0  drv_lcdc.o(i.drv_lcdc_cfg_int_frame)
    i.drv_lcdc_clear_int                     0x000137f0   Section        0  drv_lcdc.o(i.drv_lcdc_clear_int)
    drv_lcdc_clear_int                       0x000137f1   Thumb Code    20  drv_lcdc.o(i.drv_lcdc_clear_int)
    i.drv_lcdc_cmd_start                     0x00013808   Section        0  drv_lcdc.o(i.drv_lcdc_cmd_start)
    i.drv_lcdc_config_acc_command_mode       0x0001383c   Section        0  drv_lcdc.o(i.drv_lcdc_config_acc_command_mode)
    i.drv_lcdc_config_int                    0x00013850   Section        0  drv_lcdc.o(i.drv_lcdc_config_int)
    i.drv_lcdc_config_int_single             0x00013888   Section        0  drv_lcdc.o(i.drv_lcdc_config_int_single)
    i.drv_lcdc_config_overwrite_rgb          0x000138b0   Section        0  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    i.drv_lcdc_config_src_parameter          0x000138c8   Section        0  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    i.drv_lcdc_crop_hact                     0x00013918   Section        0  drv_lcdc.o(i.drv_lcdc_crop_hact)
    i.drv_lcdc_ctrl_flow                     0x00013928   Section        0  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    i.drv_lcdc_dith_config                   0x00013960   Section        0  drv_lcdc.o(i.drv_lcdc_dith_config)
    i.drv_lcdc_edge_dect_config              0x00013990   Section        0  drv_lcdc.o(i.drv_lcdc_edge_dect_config)
    i.drv_lcdc_edge_enh_config               0x000139cc   Section        0  drv_lcdc.o(i.drv_lcdc_edge_enh_config)
    i.drv_lcdc_enable_shadow_reg             0x00013a30   Section        0  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    i.drv_lcdc_endianness_config             0x00013a54   Section        0  drv_lcdc.o(i.drv_lcdc_endianness_config)
    i.drv_lcdc_fc_config                     0x00013a70   Section        0  drv_lcdc.o(i.drv_lcdc_fc_config)
    i.drv_lcdc_fldc_config                   0x00013a90   Section        0  drv_lcdc.o(i.drv_lcdc_fldc_config)
    i.drv_lcdc_function_disable              0x00013ab4   Section        0  drv_lcdc.o(i.drv_lcdc_function_disable)
    i.drv_lcdc_function_enable               0x00013ad8   Section        0  drv_lcdc.o(i.drv_lcdc_function_enable)
    i.drv_lcdc_set_int                       0x00013afc   Section        0  drv_lcdc.o(i.drv_lcdc_set_int)
    i.drv_lcdc_set_prefetch                  0x00013b38   Section        0  drv_lcdc.o(i.drv_lcdc_set_prefetch)
    i.drv_lcdc_set_tear_line                 0x00013b54   Section        0  drv_lcdc.o(i.drv_lcdc_set_tear_line)
    i.drv_lcdc_stop_display                  0x00013b70   Section        0  drv_lcdc.o(i.drv_lcdc_stop_display)
    i.drv_lcdc_vid_hw_start                  0x00013b80   Section        0  drv_lcdc.o(i.drv_lcdc_vid_hw_start)
    i.drv_lcdc_vintp_mode_config             0x00013bbc   Section        0  drv_lcdc.o(i.drv_lcdc_vintp_mode_config)
    i.drv_memc_clear_status                  0x00013bd4   Section        0  drv_memc.o(i.drv_memc_clear_status)
    i.drv_memc_enable_irq                    0x00013be8   Section        0  drv_memc.o(i.drv_memc_enable_irq)
    i.drv_memc_gen_a_tear_signal             0x00013c28   Section        0  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    i.drv_memc_get_status                    0x00013c38   Section        0  drv_memc.o(i.drv_memc_get_status)
    i.drv_memc_get_tear_mode                 0x00013c50   Section        0  drv_memc.o(i.drv_memc_get_tear_mode)
    i.drv_memc_rate_transfer_sel             0x00013c60   Section        0  drv_memc.o(i.drv_memc_rate_transfer_sel)
    i.drv_memc_sel_vsync                     0x00013c7c   Section        0  drv_memc.o(i.drv_memc_sel_vsync)
    i.drv_memc_set_active_height             0x00013c90   Section        0  drv_memc.o(i.drv_memc_set_active_height)
    i.drv_memc_set_circ_mode_enable          0x00013ca8   Section        0  drv_memc.o(i.drv_memc_set_circ_mode_enable)
    i.drv_memc_set_data_mode                 0x00013cc4   Section        0  drv_memc.o(i.drv_memc_set_data_mode)
    i.drv_memc_set_double_buffer             0x00013cd8   Section        0  drv_memc.o(i.drv_memc_set_double_buffer)
    i.drv_memc_set_frame_drop_select         0x00013cf0   Section        0  drv_memc.o(i.drv_memc_set_frame_drop_select)
    i.drv_memc_set_fs_en_conditions          0x00013d0c   Section        0  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    i.drv_memc_set_lcdc_st_conditions        0x00013d24   Section        0  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    i.drv_memc_set_ltpo_mode                 0x00013d40   Section        0  drv_memc.o(i.drv_memc_set_ltpo_mode)
    i.drv_memc_set_ltpo_pu_thres             0x00013d60   Section        0  drv_memc.o(i.drv_memc_set_ltpo_pu_thres)
    i.drv_memc_set_tear_mode                 0x00013d78   Section        0  drv_memc.o(i.drv_memc_set_tear_mode)
    i.drv_memc_set_tear_waveform             0x00013d8c   Section        0  drv_memc.o(i.drv_memc_set_tear_waveform)
    i.drv_memc_set_vidc_sync_cnt             0x00013db8   Section        0  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    i.drv_phy_test_clear                     0x00013dcc   Section        0  drv_phy_common.o(i.drv_phy_test_clear)
    i.drv_phy_test_lock                      0x00013ddc   Section        0  drv_phy_common.o(i.drv_phy_test_lock)
    i.drv_pwr_efuse_pd                       0x00013df4   Section        0  drv_pwr.o(i.drv_pwr_efuse_pd)
    i.drv_pwr_enter_deep_sleep_mode          0x00013e24   Section        0  drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode)
    i.drv_pwr_enter_sleep_mode_ex            0x00013e70   Section        0  drv_pwr.o(i.drv_pwr_enter_sleep_mode_ex)
    i.drv_pwr_enter_stop_sleep_mode          0x00013ea4   Section        0  drv_pwr.o(i.drv_pwr_enter_stop_sleep_mode)
    i.drv_pwr_exit_sleep_mode                0x00013f3c   Section        0  drv_pwr.o(i.drv_pwr_exit_sleep_mode)
    i.drv_pwr_get_power_ready_st             0x00013f64   Section        0  drv_pwr.o(i.drv_pwr_get_power_ready_st)
    i.drv_pwr_set_breath_screen_power_sel    0x00013f74   Section        0  drv_pwr.o(i.drv_pwr_set_breath_screen_power_sel)
    i.drv_pwr_set_digit_power_sel            0x00013f9c   Section        0  drv_pwr.o(i.drv_pwr_set_digit_power_sel)
    i.drv_pwr_set_pll_clk                    0x00013fc4   Section        0  drv_pwr.o(i.drv_pwr_set_pll_clk)
    i.drv_pwr_set_wakeup_type                0x00013ff8   Section        0  drv_pwr.o(i.drv_pwr_set_wakeup_type)
    i.drv_pwr_write_lock                     0x00014024   Section        0  drv_pwr.o(i.drv_pwr_write_lock)
    i.drv_rxbr_clear_pkt_buffer              0x00014044   Section        0  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    i.drv_rxbr_clear_status0                 0x00014054   Section        0  drv_rxbr.o(i.drv_rxbr_clear_status0)
    i.drv_rxbr_enable_irq                    0x00014060   Section        0  drv_rxbr.o(i.drv_rxbr_enable_irq)
    i.drv_rxbr_frame_drop_cfg                0x000140bc   Section        0  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    i.drv_rxbr_get_int_source                0x000140d8   Section        0  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    drv_rxbr_get_int_source                  0x000140d9   Thumb Code    20  hal_internal_vsync.o(i.drv_rxbr_get_int_source)
    i.drv_rxbr_get_status0                   0x000140f0   Section        0  hal_internal_dcs.o(i.drv_rxbr_get_status0)
    drv_rxbr_get_status0                     0x000140f1   Thumb Code    20  hal_internal_dcs.o(i.drv_rxbr_get_status0)
    i.drv_rxbr_hline_rcv1_cfg                0x00014108   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg)
    i.drv_rxbr_hline_rcv_cfg                 0x0001411c   Section        0  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    i.drv_rxbr_register_irq1_callback        0x0001412c   Section        0  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    i.drv_rxbr_set_cmd_response              0x00014138   Section        0  drv_rxbr.o(i.drv_rxbr_set_cmd_response)
    i.drv_rxbr_set_color_format              0x0001427c   Section        0  drv_rxbr.o(i.drv_rxbr_set_color_format)
    i.drv_rxbr_set_filter_regs               0x00014298   Section        0  drv_rxbr.o(i.drv_rxbr_set_filter_regs)
    i.drv_rxbr_set_inten                     0x000142bc   Section        0  drv_rxbr.o(i.drv_rxbr_set_inten)
    i.drv_rxbr_set_ltpo_drop_th              0x000142d8   Section        0  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    i.drv_rxbr_set_usr_cfg                   0x000142f0   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    i.drv_rxbr_set_usr_col                   0x00014330   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    i.drv_rxbr_set_usr_row                   0x00014340   Section        0  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    i.drv_se_init                            0x00014350   Section        0  drv_se.o(i.drv_se_init)
    i.drv_se_set_dsc                         0x000143c8   Section        0  drv_se.o(i.drv_se_set_dsc)
    i.drv_se_set_lcdc                        0x0001449c   Section        0  drv_se.o(i.drv_se_set_lcdc)
    i.drv_se_set_memc                        0x00014524   Section        0  drv_se.o(i.drv_se_set_memc)
    i.drv_se_set_rxbr                        0x000145b4   Section        0  drv_se.o(i.drv_se_set_rxbr)
    i.drv_se_set_vidc                        0x00014684   Section        0  drv_se.o(i.drv_se_set_vidc)
    i.drv_se_start_rx                        0x00014730   Section        0  drv_se.o(i.drv_se_start_rx)
    i.drv_spim_clear_int_status              0x00014744   Section        0  drv_spi_master.o(i.drv_spim_clear_int_status)
    i.drv_spim_disable_int                   0x00014750   Section        0  drv_spi_master.o(i.drv_spim_disable_int)
    i.drv_spim_set_inten                     0x00014780   Section        0  drv_spi_master.o(i.drv_spim_set_inten)
    i.drv_swire_enable                       0x0001479c   Section        0  drv_swire.o(i.drv_swire_enable)
    i.drv_swire_get_pulse_count              0x000147b8   Section        0  drv_swire.o(i.drv_swire_get_pulse_count)
    i.drv_swire_register_callback            0x000147c4   Section        0  drv_swire.o(i.drv_swire_register_callback)
    i.drv_swire_set_bit_time                 0x000147d0   Section        0  drv_swire.o(i.drv_swire_set_bit_time)
    i.drv_swire_set_int                      0x000147e8   Section        0  drv_swire.o(i.drv_swire_set_int)
    i.drv_swire_set_power_down               0x00014830   Section        0  drv_swire.o(i.drv_swire_set_power_down)
    i.drv_swire_set_pulse_count              0x0001484c   Section        0  drv_swire.o(i.drv_swire_set_pulse_count)
    i.drv_swire_set_trig_mode                0x00014858   Section        0  drv_swire.o(i.drv_swire_set_trig_mode)
    i.drv_sys_cfg_clear_all_int              0x00014874   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    i.drv_sys_cfg_clear_pending              0x00014880   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    i.drv_sys_cfg_sel_ap_rst_trig            0x000148a8   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig)
    i.drv_sys_cfg_sel_gpio_group             0x000148cc   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group)
    i.drv_sys_cfg_sel_int_trig               0x000148f0   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig)
    i.drv_sys_cfg_sel_swire_timer            0x00014914   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_sel_swire_timer)
    i.drv_sys_cfg_set_int                    0x0001492c   Section        0  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    i.drv_timer_clear_status_flags           0x00014950   Section        0  drv_timer.o(i.drv_timer_clear_status_flags)
    drv_timer_clear_status_flags             0x00014951   Thumb Code    26  drv_timer.o(i.drv_timer_clear_status_flags)
    i.drv_timer_enable                       0x0001496a   Section        0  drv_timer.o(i.drv_timer_enable)
    i.drv_timer_get_instance                 0x0001498c   Section        0  drv_timer.o(i.drv_timer_get_instance)
    i.drv_timer_handle_interrupt             0x0001499c   Section        0  drv_timer.o(i.drv_timer_handle_interrupt)
    drv_timer_handle_interrupt               0x0001499d   Thumb Code    54  drv_timer.o(i.drv_timer_handle_interrupt)
    i.drv_timer_register_callback            0x000149d8   Section        0  drv_timer.o(i.drv_timer_register_callback)
    i.drv_timer_set_compare_val              0x000149ec   Section        0  drv_timer.o(i.drv_timer_set_compare_val)
    i.drv_timer_set_int                      0x00014a2c   Section        0  drv_timer.o(i.drv_timer_set_int)
    i.drv_timer_set_prescaler                0x00014a74   Section        0  drv_timer.o(i.drv_timer_set_prescaler)
    i.drv_timer_set_repeat                   0x00014a9c   Section        0  drv_timer.o(i.drv_timer_set_repeat)
    i.drv_tx_phy_test_enter                  0x00014aac   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    i.drv_tx_phy_test_exit                   0x00014acc   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    i.drv_tx_phy_test_write_code             0x00014aec   Section        0  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    i.drv_uart_abort_recv                    0x00014b14   Section        0  drv_uart.o(i.drv_uart_abort_recv)
    i.drv_uart_abort_send                    0x00014b48   Section        0  drv_uart.o(i.drv_uart_abort_send)
    i.drv_uart_config_int                    0x00014b7c   Section        0  drv_uart.o(i.drv_uart_config_int)
    i.drv_uart_enable_clk                    0x00014b90   Section        0  drv_uart.o(i.drv_uart_enable_clk)
    drv_uart_enable_clk                      0x00014b91   Thumb Code    24  drv_uart.o(i.drv_uart_enable_clk)
    i.drv_uart_enable_int                    0x00014ba8   Section        0  drv_uart.o(i.drv_uart_enable_int)
    i.drv_uart_get_instance                  0x00014c04   Section        0  drv_uart.o(i.drv_uart_get_instance)
    i.drv_uart_init                          0x00014c2c   Section        0  drv_uart.o(i.drv_uart_init)
    i.drv_uart_int_trans_handle              0x00014cfc   Section        0  drv_uart.o(i.drv_uart_int_trans_handle)
    drv_uart_int_trans_handle                0x00014cfd   Thumb Code    54  drv_uart.o(i.drv_uart_int_trans_handle)
    i.drv_uart_reset_rx_fifo                 0x00014d38   Section        0  drv_uart.o(i.drv_uart_reset_rx_fifo)
    i.drv_uart_reset_tx_fifo                 0x00014d54   Section        0  drv_uart.o(i.drv_uart_reset_tx_fifo)
    i.drv_uart_send_blocking                 0x00014d70   Section        0  drv_uart.o(i.drv_uart_send_blocking)
    i.drv_uart_set_baud_rate                 0x00014d8a   Section        0  drv_uart.o(i.drv_uart_set_baud_rate)
    i.drv_uart_trans_create_handle           0x00014de0   Section        0  drv_uart.o(i.drv_uart_trans_create_handle)
    i.drv_vidc_clear_irq                     0x00014e2c   Section        0  drv_vidc.o(i.drv_vidc_clear_irq)
    i.drv_vidc_enable                        0x00014e3c   Section        0  drv_vidc.o(i.drv_vidc_enable)
    i.drv_vidc_enable_irq                    0x00014e5c   Section        0  drv_vidc.o(i.drv_vidc_enable_irq)
    i.drv_vidc_get_int_source                0x00014e9c   Section        0  drv_vidc.o(i.drv_vidc_get_int_source)
    i.drv_vidc_get_irq_status                0x00014ec8   Section        0  drv_vidc.o(i.drv_vidc_get_irq_status)
    i.drv_vidc_init_module_enable            0x00014ee0   Section        0  drv_vidc.o(i.drv_vidc_init_module_enable)
    i.drv_vidc_register_callback             0x00014f0c   Section        0  drv_vidc.o(i.drv_vidc_register_callback)
    i.drv_vidc_reset                         0x00014f18   Section        0  drv_vidc.o(i.drv_vidc_reset)
    i.drv_vidc_set_circ_mode_enable          0x00014f24   Section        0  drv_vidc.o(i.drv_vidc_set_circ_mode_enable)
    i.drv_vidc_set_dither_config             0x00014f40   Section        0  drv_vidc.o(i.drv_vidc_set_dither_config)
    i.drv_vidc_set_dst_parameter             0x00014f78   Section        0  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    i.drv_vidc_set_honly_hcoef0              0x00014fd4   Section        0  drv_vidc.o(i.drv_vidc_set_honly_hcoef0)
    i.drv_vidc_set_honly_hinitb              0x00014fe0   Section        0  drv_vidc.o(i.drv_vidc_set_honly_hinitb)
    i.drv_vidc_set_honly_hinitr              0x0001500c   Section        0  drv_vidc.o(i.drv_vidc_set_honly_hinitr)
    i.drv_vidc_set_irqen                     0x0001503c   Section        0  drv_vidc.o(i.drv_vidc_set_irqen)
    i.drv_vidc_set_mirror                    0x00015058   Section        0  drv_vidc.o(i.drv_vidc_set_mirror)
    i.drv_vidc_set_pentile_swap              0x0001506c   Section        0  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    i.drv_vidc_set_pu_ctrl                   0x00015088   Section        0  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    i.drv_vidc_set_rotation                  0x00015094   Section        0  drv_vidc.o(i.drv_vidc_set_rotation)
    i.drv_vidc_set_scld_hcoef0               0x000150ac   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    i.drv_vidc_set_scld_hcoef1               0x000150b8   Section        0  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    i.drv_vidc_set_scld_step                 0x000150c4   Section        0  drv_vidc.o(i.drv_vidc_set_scld_step)
    i.drv_vidc_set_scld_vcoef0               0x000150d8   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    i.drv_vidc_set_scld_vcoef1               0x000150e4   Section        0  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    i.drv_vidc_set_src_parameter             0x000150f0   Section        0  drv_vidc.o(i.drv_vidc_set_src_parameter)
    i.drv_vidc_set_vintp_config              0x00015110   Section        0  drv_vidc.o(i.drv_vidc_set_vintp_config)
    i.drv_wdg_clear_counter                  0x00015148   Section        0  drv_wdg.o(i.drv_wdg_clear_counter)
    i.drv_wdg_clear_edge_flag                0x00015158   Section        0  drv_wdg.o(i.drv_wdg_clear_edge_flag)
    drv_wdg_clear_edge_flag                  0x00015159   Thumb Code    12  drv_wdg.o(i.drv_wdg_clear_edge_flag)
    i.drv_wdg_read_edge_flag                 0x00015168   Section        0  drv_wdg.o(i.drv_wdg_read_edge_flag)
    drv_wdg_read_edge_flag                   0x00015169   Thumb Code    10  drv_wdg.o(i.drv_wdg_read_edge_flag)
    i.drv_wdg_set_int                        0x00015178   Section        0  drv_wdg.o(i.drv_wdg_set_int)
    i.fputc                                  0x000151ac   Section        0  tau_log.o(i.fputc)
    i.ha_intl_fb_check_pu_size               0x000151e0   Section        0  hal_internal_fb.o(i.ha_intl_fb_check_pu_size)
    ha_intl_fb_check_pu_size                 0x000151e1   Thumb Code    58  hal_internal_fb.o(i.ha_intl_fb_check_pu_size)
    i.hal_dsi_rx_ctrl_create_handle          0x00015220   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    i.hal_dsi_rx_ctrl_dcs_async_handler      0x00015260   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler)
    i.hal_dsi_rx_ctrl_deinit                 0x000152a0   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit)
    i.hal_dsi_rx_ctrl_init                   0x00015334   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    i.hal_dsi_rx_ctrl_init_clk               0x000153e0   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    hal_dsi_rx_ctrl_init_clk                 0x000153e1   Thumb Code   222  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_clk)
    i.hal_dsi_rx_ctrl_init_dsi_rx            0x000154e0   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    hal_dsi_rx_ctrl_init_dsi_rx              0x000154e1   Thumb Code   218  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_dsi_rx)
    i.hal_dsi_rx_ctrl_init_memc              0x000155d8   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    hal_dsi_rx_ctrl_init_memc                0x000155d9   Thumb Code   294  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_memc)
    i.hal_dsi_rx_ctrl_init_rxbr              0x00015704   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    hal_dsi_rx_ctrl_init_rxbr                0x00015705   Thumb Code   314  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_rxbr)
    i.hal_dsi_rx_ctrl_init_vidc              0x0001584c   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    hal_dsi_rx_ctrl_init_vidc                0x0001584d   Thumb Code   624  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init_vidc)
    i.hal_dsi_rx_ctrl_pre_init_pps           0x00015acc   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    i.hal_dsi_rx_ctrl_set_auto_ack           0x00015b04   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack)
    i.hal_dsi_rx_ctrl_set_ipi_cfg            0x00015bb4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    hal_dsi_rx_ctrl_set_ipi_cfg              0x00015bb5   Thumb Code    48  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_ipi_cfg)
    i.hal_dsi_rx_ctrl_start                  0x00015be4   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    i.hal_dsi_rx_ctrl_stop                   0x00015c14   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop)
    i.hal_dsi_rx_ctrl_toggle_resolution      0x00015c44   Section        0  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    i.hal_dsi_tx_cmd_mode_cal_timing         0x00015c64   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing)
    hal_dsi_tx_cmd_mode_cal_timing           0x00015c65   Thumb Code   506  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_cmd_mode_cal_timing)
    i.hal_dsi_tx_ctrl_create_handle          0x00015ee0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    i.hal_dsi_tx_ctrl_deinit                 0x00015f18   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit)
    i.hal_dsi_tx_ctrl_gen_a_tear_signal      0x00015f8c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal)
    i.hal_dsi_tx_ctrl_init                   0x00015fb0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    i.hal_dsi_tx_ctrl_init_clk               0x0001602c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    hal_dsi_tx_ctrl_init_clk                 0x0001602d   Thumb Code    12  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init_clk)
    i.hal_dsi_tx_ctrl_set_overwrite_rgb      0x0001603c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    i.hal_dsi_tx_ctrl_set_tear_mode          0x00016044   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode)
    i.hal_dsi_tx_ctrl_start                  0x00016050   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    i.hal_dsi_tx_ctrl_stop                   0x000160e0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop)
    i.hal_dsi_tx_ctrl_write_array_cmd        0x00016118   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd)
    i.hal_dsi_tx_ctrl_write_cmd              0x0001620c   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    i.hal_dsi_tx_init_cfg                    0x000162dc   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg)
    hal_dsi_tx_init_cfg                      0x000162dd   Thumb Code   250  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_cfg)
    i.hal_dsi_tx_init_dpi_timing             0x000163e0   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing)
    hal_dsi_tx_init_dpi_timing               0x000163e1   Thumb Code    46  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_dpi_timing)
    i.hal_dsi_tx_init_phy_cfg                0x00016418   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    hal_dsi_tx_init_phy_cfg                  0x00016419   Thumb Code    22  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_phy_cfg)
    i.hal_dsi_tx_init_timing                 0x0001642e   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing)
    hal_dsi_tx_init_timing                   0x0001642f   Thumb Code    82  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_timing)
    i.hal_dsi_tx_init_vid_timing             0x00016480   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing)
    hal_dsi_tx_init_vid_timing               0x00016481   Thumb Code    70  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_init_vid_timing)
    i.hal_dsi_tx_send_cmd                    0x000164d4   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    hal_dsi_tx_send_cmd                      0x000164d5   Thumb Code    58  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_send_cmd)
    i.hal_dsi_tx_timing_info_update          0x00016514   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update)
    hal_dsi_tx_timing_info_update            0x00016515   Thumb Code   142  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_timing_info_update)
    i.hal_dsi_tx_vid_mode_cal_timing         0x000165a8   Section        0  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing)
    hal_dsi_tx_vid_mode_cal_timing           0x000165a9   Thumb Code   766  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_vid_mode_cal_timing)
    i.hal_gpio_config_pad                    0x000168b8   Section        0  hal_gpio.o(i.hal_gpio_config_pad)
    i.hal_gpio_ctrl_eint                     0x000168f4   Section        0  hal_gpio.o(i.hal_gpio_ctrl_eint)
    i.hal_gpio_init_eint                     0x0001690c   Section        0  hal_gpio.o(i.hal_gpio_init_eint)
    i.hal_gpio_init_input                    0x0001694c   Section        0  hal_gpio.o(i.hal_gpio_init_input)
    i.hal_gpio_init_output                   0x00016962   Section        0  hal_gpio.o(i.hal_gpio_init_output)
    i.hal_gpio_reg_eint_cb                   0x00016980   Section        0  hal_gpio.o(i.hal_gpio_reg_eint_cb)
    i.hal_gpio_set_ap_reset_int              0x0001699c   Section        0  hal_gpio.o(i.hal_gpio_set_ap_reset_int)
    i.hal_gpio_set_mode                      0x000169ec   Section        0  hal_gpio.o(i.hal_gpio_set_mode)
    i.hal_gpio_set_output_data               0x00016a4c   Section        0  hal_gpio.o(i.hal_gpio_set_output_data)
    i.hal_internal_sync_get_hight_performan_mode 0x00016a54   Section        0  hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode)
    i.hal_internal_sync_input_resolution_change 0x00016a64   Section        0  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    i.hal_internal_sync_register_lcdc_cb     0x00016c10   Section        0  hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb)
    i.hal_internal_vsync_deinit              0x00016c1c   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    i.hal_internal_vsync_get_rx_state        0x00016c3c   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state)
    i.hal_internal_vsync_get_sync_line       0x00016c48   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    i.hal_internal_vsync_get_tx_state        0x00016c5c   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    i.hal_internal_vsync_init_rx             0x00016c68   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    i.hal_internal_vsync_init_tx             0x00016d50   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    i.hal_internal_vsync_set_rx_state        0x00016e18   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    i.hal_internal_vsync_set_tear_mode       0x00016e38   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    i.hal_internal_vsync_set_tx_state        0x00016f7c   Section        0  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    i.hal_intl_dcs_init_sw_fltr              0x00016fd4   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr)
    i.hal_intl_dcs_rx_get_dcs_packet_data    0x00017040   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data)
    hal_intl_dcs_rx_get_dcs_packet_data      0x00017041   Thumb Code   806  hal_internal_dcs.o(i.hal_intl_dcs_rx_get_dcs_packet_data)
    i.hal_intl_dcs_rx_receive_packet         0x0001748c   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet)
    hal_intl_dcs_rx_receive_packet           0x0001748d   Thumb Code   122  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_packet)
    i.hal_intl_dcs_rx_receive_pps            0x00017514   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps)
    hal_intl_dcs_rx_receive_pps              0x00017515   Thumb Code   268  hal_internal_dcs.o(i.hal_intl_dcs_rx_receive_pps)
    i.hal_intl_dcs_set_auto_hw_filter        0x00017688   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter)
    i.hal_intl_dcs_sw_filter_handle          0x00017714   Section        0  hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle)
    hal_intl_dcs_sw_filter_handle            0x00017715   Thumb Code    36  hal_internal_dcs.o(i.hal_intl_dcs_sw_filter_handle)
    i.hal_intl_fb_cal_fb_info                0x00017740   Section        0  hal_internal_fb.o(i.hal_intl_fb_cal_fb_info)
    i.hal_intl_fb_check_bandwidth            0x00017a30   Section        0  hal_internal_fb.o(i.hal_intl_fb_check_bandwidth)
    hal_intl_fb_check_bandwidth              0x00017a31   Thumb Code    92  hal_internal_fb.o(i.hal_intl_fb_check_bandwidth)
    i.hal_intl_fb_edge_resize                0x00017a94   Section        0  hal_internal_fb.o(i.hal_intl_fb_edge_resize)
    hal_intl_fb_edge_resize                  0x00017a95   Thumb Code   214  hal_internal_fb.o(i.hal_intl_fb_edge_resize)
    i.hal_intl_fb_flow_control_adapter       0x00017b70   Section        0  hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter)
    hal_intl_fb_flow_control_adapter         0x00017b71   Thumb Code   110  hal_internal_fb.o(i.hal_intl_fb_flow_control_adapter)
    i.hal_intl_fb_get_memc_flow_mode         0x00017be4   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode)
    i.hal_intl_fb_get_rx_fb_info             0x00017bf0   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info)
    i.hal_intl_fb_get_tx_fb_info             0x00017c00   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info)
    i.hal_intl_fb_get_user_flow              0x00017c10   Section        0  hal_internal_fb.o(i.hal_intl_fb_get_user_flow)
    i.hal_intl_svs_deinit_rx                 0x00017c1c   Section        0  hal_internal_svs.o(i.hal_intl_svs_deinit_rx)
    i.hal_intl_svs_deinit_tx                 0x00017c44   Section        0  hal_internal_svs.o(i.hal_intl_svs_deinit_tx)
    i.hal_intl_svs_handle                    0x00017c54   Section        0  hal_internal_svs.o(i.hal_intl_svs_handle)
    i.hal_intl_svs_init_rx                   0x00017c78   Section        0  hal_internal_svs.o(i.hal_intl_svs_init_rx)
    i.hal_intl_svs_init_tx                   0x00017cf8   Section        0  hal_internal_svs.o(i.hal_intl_svs_init_tx)
    i.hal_intl_svs_set_rx_vtt                0x00017d0c   Section        0  hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt)
    i.hal_intl_svs_update_rxbr_clk           0x00017d18   Section        0  hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk)
    i.hal_lcdc_displayproc_config            0x00017d60   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config)
    i.hal_lcdc_init_cfg                      0x00017dd0   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    hal_lcdc_init_cfg                        0x00017dd1   Thumb Code    62  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_cfg)
    i.hal_lcdc_init_clk                      0x00017e0e   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    hal_lcdc_init_clk                        0x00017e0f   Thumb Code   112  hal_dsi_tx_ctrl.o(i.hal_lcdc_init_clk)
    i.hal_lcdc_postproc_config               0x00017e80   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config)
    i.hal_lcdc_start                         0x00017fa8   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_start)
    hal_lcdc_start                           0x00017fa9   Thumb Code    36  hal_dsi_tx_ctrl.o(i.hal_lcdc_start)
    i.hal_lcdc_timinggen_config              0x00017fcc   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config)
    hal_lcdc_timinggen_config                0x00017fcd   Thumb Code    60  hal_dsi_tx_ctrl.o(i.hal_lcdc_timinggen_config)
    i.hal_lcdc_upscaler_config               0x00018008   Section        0  hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config)
    i.hal_nonshadow_func_update              0x000180e8   Section        0  hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update)
    i.hal_pwr_enter_deep_sleep_mode          0x000181a4   Section        0  hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode)
    i.hal_pwr_enter_normal_sleep_mode        0x000181ce   Section        0  hal_pwr.o(i.hal_pwr_enter_normal_sleep_mode)
    i.hal_pwr_enter_stop_sleep_mode          0x000181d8   Section        0  hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode)
    i.hal_pwr_exit_sleep_mode                0x0001823c   Section        0  hal_pwr.o(i.hal_pwr_exit_sleep_mode)
    i.hal_pwr_get_vcc_power_ready            0x00018246   Section        0  hal_pwr.o(i.hal_pwr_get_vcc_power_ready)
    i.hal_pwr_set_main_power                 0x0001824e   Section        0  hal_pwr.o(i.hal_pwr_set_main_power)
    i.hal_pwr_set_sleep_mode_power           0x00018256   Section        0  hal_pwr.o(i.hal_pwr_set_sleep_mode_power)
    i.hal_pwr_set_stop_sleep_wakeup_pin      0x00018260   Section        0  hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin)
    i.hal_swire_deinit                       0x000182c4   Section        0  hal_swire.o(i.hal_swire_deinit)
    i.hal_swire_enable                       0x00018304   Section        0  hal_swire.o(i.hal_swire_enable)
    i.hal_swire_init                         0x00018360   Section        0  hal_swire.o(i.hal_swire_init)
    i.hal_swire_set_pulse                    0x000183b8   Section        0  hal_swire.o(i.hal_swire_set_pulse)
    i.hal_swire_set_timer                    0x000183dc   Section        0  hal_swire.o(i.hal_swire_set_timer)
    i.hal_system_init                        0x0001841c   Section        0  hal_system.o(i.hal_system_init)
    i.hal_system_updata_sysclk               0x00018500   Section        0  hal_system.o(i.hal_system_updata_sysclk)
    i.hal_timer_deinit                       0x00018550   Section        0  hal_timer.o(i.hal_timer_deinit)
    i.hal_timer_init                         0x00018580   Section        0  hal_timer.o(i.hal_timer_init)
    i.hal_timer_set_repeat                   0x0001859c   Section        0  hal_timer.o(i.hal_timer_set_repeat)
    i.hal_timer_start                        0x000185a4   Section        0  hal_timer.o(i.hal_timer_start)
    i.hal_timer_stop                         0x000185d4   Section        0  hal_timer.o(i.hal_timer_stop)
    i.hal_tx_frame_rate_adjust               0x000185fc   Section        0  hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust)
    hal_tx_frame_rate_adjust                 0x000185fd   Thumb Code    44  hal_dsi_tx_ctrl.o(i.hal_tx_frame_rate_adjust)
    i.hal_uart_init                          0x0001862c   Section        0  hal_uart.o(i.hal_uart_init)
    i.hal_uart_send_blocking                 0x000186c0   Section        0  hal_uart.o(i.hal_uart_send_blocking)
    i.hal_vsync_func_update                  0x000186dc   Section        0  hal_dsi_tx_ctrl.o(i.hal_vsync_func_update)
    i.hal_vsync_reset_lcdc_scaler            0x000186f4   Section        0  hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler)
    i.main                                   0x000187d4   Section        0  main.o(i.main)
    i.pps_update_handle                      0x00018814   Section        0  s8_demo.o(i.pps_update_handle)
    pps_update_handle                        0x00018815   Thumb Code    76  s8_demo.o(i.pps_update_handle)
    i.rxbr_irq1_callback                     0x00018868   Section        0  hal_internal_vsync.o(i.rxbr_irq1_callback)
    rxbr_irq1_callback                       0x00018869   Thumb Code   478  hal_internal_vsync.o(i.rxbr_irq1_callback)
    i.s8_demo                                0x00018b4c   Section        0  s8_demo.o(i.s8_demo)
    i.send_panel_init_code                   0x00018bac   Section        0  s8_demo.o(i.send_panel_init_code)
    send_panel_init_code                     0x00018bad   Thumb Code    58  s8_demo.o(i.send_panel_init_code)
    i.soft_double_buffer_update              0x00018be8   Section        0  hal_internal_vsync.o(i.soft_double_buffer_update)
    soft_double_buffer_update                0x00018be9   Thumb Code    56  hal_internal_vsync.o(i.soft_double_buffer_update)
    i.soft_gen_te                            0x00018c2c   Section        0  hal_internal_vsync.o(i.soft_gen_te)
    soft_gen_te                              0x00018c2d   Thumb Code    86  hal_internal_vsync.o(i.soft_gen_te)
    i.soft_gen_te_double_buffer              0x00018c98   Section        0  hal_internal_vsync.o(i.soft_gen_te_double_buffer)
    soft_gen_te_double_buffer                0x00018c99   Thumb Code   202  hal_internal_vsync.o(i.soft_gen_te_double_buffer)
    i.soft_pro_motion_init                   0x00018d78   Section        0  hal_internal_vsync.o(i.soft_pro_motion_init)
    soft_pro_motion_init                     0x00018d79   Thumb Code    46  hal_internal_vsync.o(i.soft_pro_motion_init)
    i.soft_swire_init                        0x00018db0   Section        0  s8_demo.o(i.soft_swire_init)
    soft_swire_init                          0x00018db1   Thumb Code    48  s8_demo.o(i.soft_swire_init)
    i.soft_swire_start                       0x00018de8   Section        0  s8_demo.o(i.soft_swire_start)
    soft_swire_start                         0x00018de9   Thumb Code    46  s8_demo.o(i.soft_swire_start)
    i.soft_swire_timer_callback              0x00018e18   Section        0  s8_demo.o(i.soft_swire_timer_callback)
    soft_swire_timer_callback                0x00018e19   Thumb Code    64  s8_demo.o(i.soft_swire_timer_callback)
    i.soft_tear_adjust_line                  0x00018e60   Section        0  hal_internal_vsync.o(i.soft_tear_adjust_line)
    soft_tear_adjust_line                    0x00018e61   Thumb Code    26  hal_internal_vsync.o(i.soft_tear_adjust_line)
    i.stop_sleep_cb                          0x00018e84   Section        0  hal_pwr.o(i.stop_sleep_cb)
    stop_sleep_cb                            0x00018e85   Thumb Code    18  hal_pwr.o(i.stop_sleep_cb)
    i.svs_direct_mode_setting                0x00018e9c   Section        0  hal_internal_svs.o(i.svs_direct_mode_setting)
    svs_direct_mode_setting                  0x00018e9d   Thumb Code   154  hal_internal_svs.o(i.svs_direct_mode_setting)
    i.svs_get_rel_intv                       0x00018f48   Section        0  hal_internal_svs.o(i.svs_get_rel_intv)
    svs_get_rel_intv                         0x00018f49   Thumb Code    20  hal_internal_svs.o(i.svs_get_rel_intv)
    i.svs_sync_handle                        0x00018f64   Section        0  hal_internal_svs.o(i.svs_sync_handle)
    svs_sync_handle                          0x00018f65   Thumb Code   158  hal_internal_svs.o(i.svs_sync_handle)
    i.svs_wait_fr_stab                       0x00019014   Section        0  hal_internal_svs.o(i.svs_wait_fr_stab)
    svs_wait_fr_stab                         0x00019015   Thumb Code   148  hal_internal_svs.o(i.svs_wait_fr_stab)
    i.svs_wait_start                         0x000190e0   Section        0  hal_internal_svs.o(i.svs_wait_start)
    svs_wait_start                           0x000190e1   Thumb Code   250  hal_internal_svs.o(i.svs_wait_start)
    i.tau_log_init                           0x000191ec   Section        0  tau_log.o(i.tau_log_init)
    i.tau_log_printf                         0x00019220   Section        0  tau_log.o(i.tau_log_printf)
    i.tau_log_push_log                       0x000192a4   Section        0  tau_log.o(i.tau_log_push_log)
    i.vidc_callback                          0x0001931c   Section        0  hal_internal_vsync.o(i.vidc_callback)
    vidc_callback                            0x0001931d   Thumb Code   150  hal_internal_vsync.o(i.vidc_callback)
    i.vpre_err_reset                         0x000193d0   Section        0  hal_internal_vsync.o(i.vpre_err_reset)
    vpre_err_reset                           0x000193d1   Thumb Code   254  hal_internal_vsync.o(i.vpre_err_reset)
    .constdata                               0x000194e8   Section     7932  s8_demo.o(.constdata)
    g_cus_rx_dcs_execute_table               0x000194e8   Data          96  s8_demo.o(.constdata)
    .constdata                               0x0001b3e4   Section       40  hal_dsi_rx_ctrl.o(.constdata)
    .constdata                               0x0001b40c   Section       28  hal_dsi_tx_ctrl.o(.constdata)
    .constdata                               0x0001b428   Section      182  hal_gpio.o(.constdata)
    s_gpio_map                               0x0001b428   Data         104  hal_gpio.o(.constdata)
    s_gpio_perf                              0x0001b490   Data          78  hal_gpio.o(.constdata)
    .constdata                               0x0001b4e0   Section       48  hal_uart.o(.constdata)
    .constdata                               0x0001b510   Section       16  drv_uart.o(.constdata)
    .conststring                             0x0001b520   Section      135  hal_dsi_rx_ctrl.o(.conststring)
    .conststring                             0x0001b5a8   Section      144  hal_internal_vsync.o(.conststring)
    .conststring                             0x0001b638   Section      142  hal_internal_dcs.o(.conststring)
    .data                                    0x00070000   Section      143  s8_demo.o(.data)
    g_rx_ctrl_handle                         0x00070000   Data           4  s8_demo.o(.data)
    g_tx_ctrl_handle                         0x00070004   Data           4  s8_demo.o(.data)
    panel_display_done                       0x00070008   Data           1  s8_demo.o(.data)
    sg_system_resume                         0x00070009   Data           1  s8_demo.o(.data)
    sg_system_suspend                        0x0007000a   Data           1  s8_demo.o(.data)
    AP_REG51_7FF                             0x0007000b   Data           1  s8_demo.o(.data)
    sg_tx_start_in_process                   0x0007000c   Data           1  s8_demo.o(.data)
    FrameRateBackUp                          0x0007008e   Data           1  s8_demo.o(.data)
    .data                                    0x00070090   Section       36  hal_dsi_rx_ctrl.o(.data)
    g_hw_auto_filter                         0x00070090   Data           1  hal_dsi_rx_ctrl.o(.data)
    g_crc_check_enable                       0x00070091   Data           1  hal_dsi_rx_ctrl.o(.data)
    g_esc_clk                                0x00070094   Data           4  hal_dsi_rx_ctrl.o(.data)
    g_before_draw_col                        0x00070098   Data           4  hal_dsi_rx_ctrl.o(.data)
    g_before_draw_page                       0x0007009c   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_step                                 0x000700a0   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_cmd_filter                           0x000700a4   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_x                                    0x000700a8   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_y                                    0x000700ac   Data           4  hal_dsi_rx_ctrl.o(.data)
    pre_value                                0x000700b0   Data           4  hal_dsi_rx_ctrl.o(.data)
    .data                                    0x000700b4   Section       92  hal_dsi_tx_ctrl.o(.data)
    sg_bta_vsync_flag                        0x000700b4   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_vsync_flag                            0x000700b5   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_enter_sleep_cmd                       0x000700b6   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_fldc_cg_mode                          0x000700b7   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_scl_fir                        0x000700b8   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_honly_bypass_fir                      0x000700b9   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_bcs                            0x000700ba   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_enhc                           0x000700bb   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_edge_dect                      0x000700bc   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_edge_enh                       0x000700bd   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_bypass_dith                           0x000700be   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_dith_judge                            0x000700bf   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_endianness                            0x000700c0   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_test_pattern_en                       0x000700c1   Data           1  hal_dsi_tx_ctrl.o(.data)
    sg_dith_judge_thr                        0x000700c4   Data           4  hal_dsi_tx_ctrl.o(.data)
    sg_ccm_para                              0x000700c8   Data          36  hal_dsi_tx_ctrl.o(.data)
    sg_honly_para                            0x000700ec   Data          36  hal_dsi_tx_ctrl.o(.data)
    .data                                    0x00070110   Section        1  hal_spi_master.o(.data)
    sg_spim_trans_end                        0x00070110   Data           1  hal_spi_master.o(.data)
    .data                                    0x00070111   Section        2  hal_swire.o(.data)
    sg_swire_timer                           0x00070111   Data           1  hal_swire.o(.data)
    sg_swire_repeat                          0x00070112   Data           1  hal_swire.o(.data)
    .data                                    0x00070114   Section        8  hal_pwr.o(.data)
    sg_wake_up_io                            0x00070114   Data           1  hal_pwr.o(.data)
    sg_stop_sleep_wakeup_int                 0x00070118   Data           4  hal_pwr.o(.data)
    .data                                    0x0007011c   Section        1  tau_log.o(.data)
    g_log_port                               0x0007011c   Data           1  tau_log.o(.data)
    .data                                    0x00070120   Section       24  hal_uart.o(.data)
    sg_dma_callback                          0x00070130   Data           4  hal_uart.o(.data)
    sg_user_data                             0x00070134   Data           4  hal_uart.o(.data)
    .data                                    0x00070138   Section       16  hal_internal_vsync.o(.data)
    s_te_refine_mode                         0x00070138   Data           1  hal_internal_vsync.o(.data)
    .data                                    0x00070148   Section       36  hal_internal_dcs.o(.data)
    g_imm_packet                             0x00070148   Data          24  hal_internal_dcs.o(.data)
    g_cus_rx_write_cmd_handle                0x00070160   Data          12  hal_internal_dcs.o(.data)
    .data                                    0x0007016c   Section       12  drv_common.o(.data)
    s_my_tick                                0x0007016c   Data           4  drv_common.o(.data)
    .data                                    0x00070178   Section        1  drv_common.o(.data)
    .data                                    0x0007017c   Section      400  drv_dma.o(.data)
    sg_dma_handle                            0x0007017c   Data         256  drv_dma.o(.data)
    .data                                    0x0007030c   Section        4  drv_gpio.o(.data)
    g_ap_reset_cb                            0x0007030c   Data           4  drv_gpio.o(.data)
    .data                                    0x00070310   Section        4  drv_swire.o(.data)
    sg_drv_swire_cb                          0x00070310   Data           4  drv_swire.o(.data)
    .data                                    0x00070314   Section       80  drv_timer.o(.data)
    sg_timer_info                            0x00070314   Data          80  drv_timer.o(.data)
    .data                                    0x00070364   Section       12  drv_wdg.o(.data)
    sg_wdg_repeat                            0x00070364   Data           1  drv_wdg.o(.data)
    sg_wdg_cb                                0x00070368   Data           8  drv_wdg.o(.data)
    .data                                    0x00070370   Section       36  drv_i2c.o(.data)
    .data                                    0x00070394   Section        4  drv_se.o(.data)
    chip_info                                0x00070394   Data           4  drv_se.o(.data)
    .data                                    0x00070398   Section        1  drv_dsi_rx.o(.data)
    sg_rx_drv_level                          0x00070398   Data           1  drv_dsi_rx.o(.data)
    .data                                    0x0007039c   Section        8  drv_rxbr.o(.data)
    .data                                    0x000703a4   Section        4  drv_vidc.o(.data)
    .data                                    0x000703a8   Section        4  stdout.o(.data)
    .bss                                     0x000703ac   Section      208  hal_dsi_rx_ctrl.o(.bss)
    g_rx_ctrl_handle                         0x000703ac   Data         208  hal_dsi_rx_ctrl.o(.bss)
    .bss                                     0x0007047c   Section      184  hal_dsi_tx_ctrl.o(.bss)
    g_tx_ctrl_handle                         0x0007047c   Data          92  hal_dsi_tx_ctrl.o(.bss)
    sg_dsi_tx_param                          0x000704d8   Data          92  hal_dsi_tx_ctrl.o(.bss)
    .bss                                     0x00070534   Section      256  tau_log.o(.bss)
    g_log_buf                                0x00070534   Data         256  tau_log.o(.bss)
    .bss                                     0x00070634   Section       68  hal_internal_vsync.o(.bss)
    .bss                                     0x00070678   Section     2048  hal_internal_dcs.o(.bss)
    .bss                                     0x00070e78   Section      255  hal_internal_dcs.o(.bss)
    g_imm_buffer                             0x00070e78   Data         255  hal_internal_dcs.o(.bss)
    .bss                                     0x00070f78   Section       68  hal_internal_fb.o(.bss)
    .bss                                     0x00070fbc   Section       68  hal_internal_svs.o(.bss)
    sg_sys_handler                           0x00070fbc   Data          68  hal_internal_svs.o(.bss)
    .bss                                     0x00071000   Section       16  drv_dma.o(.bss)
    sg_dma_int_list                          0x00071000   Data          16  drv_dma.o(.bss)
    .bss                                     0x00071010   Section       64  drv_gpio.o(.bss)
    s_gpio_cb                                0x00071010   Data          64  drv_gpio.o(.bss)
    .bss                                     0x00071050   Section     4204  dcs_packet_fifo.o(.bss)
    .bss                                     0x000720bc   Section       96  drv_uart.o(.bss)
    sg_uart_userdata                         0x000720bc   Data          96  drv_uart.o(.bss)
    STACK                                    0x00072120   Section     4096  startup_armcm0.o(STACK)

    Global Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    BuildAttributes$$THM_ISAv3M$S$PE$A:L22$X:L11$S22$IEEE1$IW$USESV6$~STKCKD$USESV7$~SHL$OTIME$ROPI$IEEEJ$EBA8$MICROLIB$REQ8$PRES8$EABIv2 0x00000000   Number         0  anon$$obj.o ABSOLUTE
    __ARM_use_no_argv                        0x00000000   Number         0  main.o ABSOLUTE
    _printf_a                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_c                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_charcount                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_d                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_e                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_f                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_flags                            0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_dec                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_hex                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_g                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_i                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_int_dec                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_l                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ll                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lld                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lli                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llo                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llu                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llx                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_dec                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_hex                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_oct                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ls                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_mbtowc                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_n                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_o                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_p                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_percent                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_pre_padding                      0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_return_value                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_s                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_sizespec                         0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_str                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_signed                  0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_unsigned                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_u                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wctomb                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_widthprec                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_x                                0x00000000   Number         0  stubs.o ABSOLUTE
    __cpp_initialize__aeabi_                  - Undefined Weak Reference
    __cxa_finalize                            - Undefined Weak Reference
    _clock_init                               - Undefined Weak Reference
    _microlib_exit                            - Undefined Weak Reference
    __Vectors_Size                           0x000000c0   Number         0  startup_armcm0.o ABSOLUTE
    __Vectors                                0x00010000   Data           4  startup_armcm0.o(RESET)
    __Vectors_End                            0x000100c0   Data           0  startup_armcm0.o(RESET)
    __main                                   0x000100c1   Thumb Code     0  entry.o(.ARM.Collect$$$$00000000)
    _main_stk                                0x000100c1   Thumb Code     0  entry2.o(.ARM.Collect$$$$00000001)
    _main_scatterload                        0x000100c5   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    __main_after_scatterload                 0x000100c9   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    _main_clock                              0x000100c9   Thumb Code     0  entry7b.o(.ARM.Collect$$$$00000008)
    _main_cpp_init                           0x000100c9   Thumb Code     0  entry8b.o(.ARM.Collect$$$$0000000A)
    _main_init                               0x000100c9   Thumb Code     0  entry9a.o(.ARM.Collect$$$$0000000B)
    __rt_final_cpp                           0x000100d1   Thumb Code     0  entry10a.o(.ARM.Collect$$$$0000000D)
    __rt_final_exit                          0x000100d1   Thumb Code     0  entry11a.o(.ARM.Collect$$$$0000000F)
    Reset_Handler                            0x000100d5   Thumb Code    28  startup_armcm0.o(.text)
    NMI_Handler                              0x000100f1   Thumb Code     2  startup_armcm0.o(.text)
    SVC_Handler                              0x000100f5   Thumb Code     2  startup_armcm0.o(.text)
    PendSV_Handler                           0x000100f7   Thumb Code     2  startup_armcm0.o(.text)
    FLSCTRL_IRQn_Handler                     0x00010107   Thumb Code     2  startup_armcm0.o(.text)
    SPIS_IRQn_Handler                        0x0001011b   Thumb Code     2  startup_armcm0.o(.text)
    OTP_IRQn_Handler                         0x00010123   Thumb Code     2  startup_armcm0.o(.text)
    PVD_IRQn_Handler                         0x00010127   Thumb Code     2  startup_armcm0.o(.text)
    __aeabi_uidiv                            0x0001014d   Thumb Code     0  uidiv.o(.text)
    __aeabi_uidivmod                         0x0001014d   Thumb Code    44  uidiv.o(.text)
    __aeabi_idiv                             0x00010179   Thumb Code     0  idiv.o(.text)
    __aeabi_idivmod                          0x00010179   Thumb Code    40  idiv.o(.text)
    __aeabi_memcpy                           0x000101a1   Thumb Code    36  memcpya.o(.text)
    __aeabi_memcpy4                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memcpy8                          0x000101a1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memset                           0x000101c5   Thumb Code    14  memseta.o(.text)
    __aeabi_memset4                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memset8                          0x000101c5   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr                           0x000101d3   Thumb Code     4  memseta.o(.text)
    __aeabi_memclr4                          0x000101d3   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr8                          0x000101d3   Thumb Code     0  memseta.o(.text)
    _memset$wrapper                          0x000101d7   Thumb Code    18  memseta.o(.text)
    strlen                                   0x000101e9   Thumb Code    14  strlen.o(.text)
    __aeabi_fadd                             0x000101f7   Thumb Code   162  fadd.o(.text)
    __aeabi_fsub                             0x00010299   Thumb Code     8  fadd.o(.text)
    __aeabi_frsub                            0x000102a1   Thumb Code     8  fadd.o(.text)
    __aeabi_fmul                             0x000102a9   Thumb Code   122  fmul.o(.text)
    __aeabi_fdiv                             0x00010323   Thumb Code   124  fdiv.o(.text)
    __ARM_scalbnf                            0x0001039f   Thumb Code    24  fscalb.o(.text)
    scalbnf                                  0x0001039f   Thumb Code     0  fscalb.o(.text)
    __aeabi_dadd                             0x000103b9   Thumb Code   328  dadd.o(.text)
    __aeabi_dsub                             0x00010501   Thumb Code    12  dadd.o(.text)
    __aeabi_drsub                            0x0001050d   Thumb Code    12  dadd.o(.text)
    __aeabi_dmul                             0x0001051d   Thumb Code   202  dmul.o(.text)
    __aeabi_ddiv                             0x000105ed   Thumb Code   234  ddiv.o(.text)
    __aeabi_ui2f                             0x000106dd   Thumb Code    14  ffltui.o(.text)
    __aeabi_ui2d                             0x000106ed   Thumb Code    24  dfltui.o(.text)
    __aeabi_f2uiz                            0x00010709   Thumb Code    40  ffixui.o(.text)
    __aeabi_d2uiz                            0x00010731   Thumb Code    50  dfixui.o(.text)
    __aeabi_f2d                              0x0001076d   Thumb Code    40  f2d.o(.text)
    __aeabi_d2f                              0x00010795   Thumb Code    56  d2f.o(.text)
    __aeabi_cfcmpeq                          0x000107cd   Thumb Code     0  cfcmple.o(.text)
    __aeabi_cfcmple                          0x000107cd   Thumb Code    20  cfcmple.o(.text)
    __aeabi_cfrcmple                         0x000107e1   Thumb Code    20  cfrcmple.o(.text)
    __aeabi_uldivmod                         0x000107f5   Thumb Code    96  uldiv.o(.text)
    __aeabi_llsl                             0x00010855   Thumb Code    32  llshl.o(.text)
    _ll_shift_l                              0x00010855   Thumb Code     0  llshl.o(.text)
    __aeabi_llsr                             0x00010875   Thumb Code    34  llushr.o(.text)
    _ll_ushift_r                             0x00010875   Thumb Code     0  llushr.o(.text)
    __aeabi_lasr                             0x00010897   Thumb Code    38  llsshr.o(.text)
    _ll_sshift_r                             0x00010897   Thumb Code     0  llsshr.o(.text)
    __I$use$fp                               0x000108bd   Thumb Code     0  iusefp.o(.text)
    _float_round                             0x000108bd   Thumb Code    16  fepilogue.o(.text)
    _float_epilogue                          0x000108cd   Thumb Code   114  fepilogue.o(.text)
    _double_round                            0x0001093f   Thumb Code    26  depilogue.o(.text)
    _double_epilogue                         0x00010959   Thumb Code   164  depilogue.o(.text)
    __aeabi_d2ulz                            0x000109fd   Thumb Code    54  dfixul.o(.text)
    __aeabi_cdrcmple                         0x00010a3d   Thumb Code    38  cdrcmple.o(.text)
    __scatterload                            0x00010a65   Thumb Code    28  init.o(.text)
    __scatterload_rt2                        0x00010a65   Thumb Code     0  init.o(.text)
    __decompress                             0x00010a89   Thumb Code     0  __dczerorl2.o(.text)
    __decompress1                            0x00010a89   Thumb Code    86  __dczerorl2.o(.text)
    AP_NRESET_IRQn_Handler                   0x00010ae1   Thumb Code    22  drv_gpio.o(i.AP_NRESET_IRQn_Handler)
    DMA_IRQn_Handler                         0x00010afd   Thumb Code    78  drv_dma.o(i.DMA_IRQn_Handler)
    EXTI_INT0_IRQn_Handler                   0x00010b59   Thumb Code    10  drv_gpio.o(i.EXTI_INT0_IRQn_Handler)
    EXTI_INT1_IRQn_Handler                   0x00010b63   Thumb Code    10  drv_gpio.o(i.EXTI_INT1_IRQn_Handler)
    EXTI_INT2_IRQn_Handler                   0x00010b6d   Thumb Code    10  drv_gpio.o(i.EXTI_INT2_IRQn_Handler)
    EXTI_INT3_IRQn_Handler                   0x00010b77   Thumb Code    10  drv_gpio.o(i.EXTI_INT3_IRQn_Handler)
    EXTI_INT4_IRQn_Handler                   0x00010b81   Thumb Code    10  drv_gpio.o(i.EXTI_INT4_IRQn_Handler)
    EXTI_INT5_IRQn_Handler                   0x00010b8b   Thumb Code    10  drv_gpio.o(i.EXTI_INT5_IRQn_Handler)
    EXTI_INT6_IRQn_Handler                   0x00010b95   Thumb Code    10  drv_gpio.o(i.EXTI_INT6_IRQn_Handler)
    EXTI_INT7_IRQn_Handler                   0x00010b9f   Thumb Code    10  drv_gpio.o(i.EXTI_INT7_IRQn_Handler)
    HardFault_Handler                        0x00010ba9   Thumb Code    14  drv_common.o(i.HardFault_Handler)
    I2C0_IRQn_Handler                        0x00010bf1   Thumb Code     8  drv_i2c.o(i.I2C0_IRQn_Handler)
    I2C1_IRQn_Handler                        0x00010bfd   Thumb Code     8  drv_i2c.o(i.I2C1_IRQn_Handler)
    I2C2_IRQn_Handler                        0x00010c09   Thumb Code     8  drv_i2c.o(i.I2C2_IRQn_Handler)
    LCDC_IRQn_Handler                        0x00010c15   Thumb Code   118  hal_internal_vsync.o(i.LCDC_IRQn_Handler)
    MEMC_IRQn_Handler                        0x00010d15   Thumb Code   154  drv_memc.o(i.MEMC_IRQn_Handler)
    MIPI_TX_IRQn_Handler                     0x00010db1   Thumb Code    70  drv_dsi_tx.o(i.MIPI_TX_IRQn_Handler)
    SPIM_IRQn_Handler                        0x00010e69   Thumb Code    62  hal_spi_master.o(i.SPIM_IRQn_Handler)
    SWIRE_IRQn_Handler                       0x00010eb1   Thumb Code    38  drv_swire.o(i.SWIRE_IRQn_Handler)
    SysTick_Handler                          0x00010ee1   Thumb Code    20  drv_common.o(i.SysTick_Handler)
    TIMER0_IRQn_Handler                      0x00010ef9   Thumb Code    10  drv_timer.o(i.TIMER0_IRQn_Handler)
    TIMER1_IRQn_Handler                      0x00010f03   Thumb Code    10  drv_timer.o(i.TIMER1_IRQn_Handler)
    TIMER2_IRQn_Handler                      0x00010f0d   Thumb Code    10  drv_timer.o(i.TIMER2_IRQn_Handler)
    TIMER3_IRQn_Handler                      0x00010f17   Thumb Code    10  drv_timer.o(i.TIMER3_IRQn_Handler)
    VIDC_IRQn_Handler                        0x00010f21   Thumb Code    22  drv_vidc.o(i.VIDC_IRQn_Handler)
    VPRE1_IRQn_Handler                       0x00010f3d   Thumb Code    22  drv_rxbr.o(i.VPRE1_IRQn_Handler)
    VPRE_IRQn_Handler                        0x00010f59   Thumb Code   104  hal_internal_dcs.o(i.VPRE_IRQn_Handler)
    WDG_IRQn_Handler                         0x00010fc5   Thumb Code    52  drv_wdg.o(i.WDG_IRQn_Handler)
    __scatterload_null                       0x00010ffd   Thumb Code     2  handlers.o(i.__scatterload_null)
    s_RAM_CK                                 0x00011000   Data          28  drv_common.o(.ARM.__at_0x11000)
    g_tau_log                                0x0001101c   Data          16  tau_log.o(.ARM.__at_0x1101C)
    sg_pq_para                               0x0001102c   Data          22  hal_dsi_tx_ctrl.o(.ARM.__at_0x1102C)
    MIPI_RX_IRQn_Handler                     0x00011045   Thumb Code   354  drv_dsi_rx.o(i.MIPI_RX_IRQn_Handler)
    UART_IRQn_Handler                        0x000113a9   Thumb Code   364  drv_uart.o(i.UART_IRQn_Handler)
    __0printf                                0x00011529   Thumb Code    24  printfa.o(i.__0printf)
    __1printf                                0x00011529   Thumb Code     0  printfa.o(i.__0printf)
    __2printf                                0x00011529   Thumb Code     0  printfa.o(i.__0printf)
    __c89printf                              0x00011529   Thumb Code     0  printfa.o(i.__0printf)
    printf                                   0x00011529   Thumb Code     0  printfa.o(i.__0printf)
    __0vsprintf                              0x00011549   Thumb Code    30  printfa.o(i.__0vsprintf)
    __1vsprintf                              0x00011549   Thumb Code     0  printfa.o(i.__0vsprintf)
    __2vsprintf                              0x00011549   Thumb Code     0  printfa.o(i.__0vsprintf)
    __c89vsprintf                            0x00011549   Thumb Code     0  printfa.o(i.__0vsprintf)
    vsprintf                                 0x00011549   Thumb Code     0  printfa.o(i.__0vsprintf)
    __ARM_clz                                0x0001156d   Thumb Code    46  depilogue.o(i.__ARM_clz)
    __ARM_common_switch8                     0x0001159b   Thumb Code    26  hal_dsi_rx_ctrl.o(i.__ARM_common_switch8)
    __scatterload_copy                       0x000115ed   Thumb Code    14  handlers.o(i.__scatterload_copy)
    __scatterload_zeroinit                   0x000115fb   Thumb Code    14  handlers.o(i.__scatterload_zeroinit)
    app_display_init                         0x000121c1   Thumb Code    58  s8_demo.o(i.app_display_init)
    app_gpio_init                            0x00012229   Thumb Code    28  s8_demo.o(i.app_gpio_init)
    board_Init                               0x00012719   Thumb Code    20  board.o(i.board_Init)
    ceil                                     0x00012731   Thumb Code   180  ceil.o(i.ceil)
    dcs_packet_fifo_alloc                    0x000128ad   Thumb Code    80  dcs_packet_fifo.o(i.dcs_packet_fifo_alloc)
    dcs_packet_fifo_init                     0x00012905   Thumb Code    18  dcs_packet_fifo.o(i.dcs_packet_fifo_init)
    dcs_packet_free_fifo_header              0x0001291d   Thumb Code    60  dcs_packet_fifo.o(i.dcs_packet_free_fifo_header)
    dcs_packet_get_fifo_header               0x00012961   Thumb Code    26  dcs_packet_fifo.o(i.dcs_packet_get_fifo_header)
    delayMs                                  0x00012985   Thumb Code    24  tau_delay.o(i.delayMs)
    delayUs                                  0x0001299d   Thumb Code    40  tau_delay.o(i.delayUs)
    drv_common_system_init                   0x000129c9   Thumb Code     8  drv_common.o(i.drv_common_system_init)
    drv_crgu_enable_clock                    0x000129d1   Thumb Code    54  drv_crgu.o(i.drv_crgu_enable_clock)
    drv_crgu_get_rxbr_clk                    0x00012a0d   Thumb Code    70  drv_crgu.o(i.drv_crgu_get_rxbr_clk)
    drv_crgu_reset_modules                   0x00012a75   Thumb Code    10  drv_crgu.o(i.drv_crgu_reset_modules)
    drv_crgu_set_ahb_clk                     0x00012a85   Thumb Code    34  drv_crgu.o(i.drv_crgu_set_ahb_clk)
    drv_crgu_set_clock_div                   0x00012aad   Thumb Code    12  drv_crgu.o(i.drv_crgu_set_clock_div)
    drv_crgu_set_dpi_clk                     0x00012abd   Thumb Code    54  drv_crgu.o(i.drv_crgu_set_dpi_clk)
    drv_crgu_set_dsc_clk                     0x00012af9   Thumb Code    52  drv_crgu.o(i.drv_crgu_set_dsc_clk)
    drv_crgu_set_fb_clk                      0x00012b31   Thumb Code    34  drv_crgu.o(i.drv_crgu_set_fb_clk)
    drv_crgu_set_lcdc_clk                    0x00012b59   Thumb Code    36  drv_crgu.o(i.drv_crgu_set_lcdc_clk)
    drv_crgu_set_reset                       0x00012b81   Thumb Code    20  drv_crgu.o(i.drv_crgu_set_reset)
    drv_crgu_set_rxbr_clk                    0x00012b99   Thumb Code    34  drv_crgu.o(i.drv_crgu_set_rxbr_clk)
    drv_crgu_set_vidc_clk                    0x00012bc1   Thumb Code    36  drv_crgu.o(i.drv_crgu_set_vidc_clk)
    drv_dma_clear_status                     0x00012be9   Thumb Code    20  drv_dma.o(i.drv_dma_clear_status)
    drv_dsc_dec_disable                      0x00012c15   Thumb Code    20  drv_dsc_dec.o(i.drv_dsc_dec_disable)
    drv_dsc_dec_enable                       0x00012c31   Thumb Code    44  drv_dsc_dec.o(i.drv_dsc_dec_enable)
    drv_dsc_dec_get_nslc                     0x00012c69   Thumb Code    22  drv_dsc_dec.o(i.drv_dsc_dec_get_nslc)
    drv_dsc_dec_set_irqen                    0x00012c89   Thumb Code    24  drv_dsc_dec.o(i.drv_dsc_dec_set_irqen)
    drv_dsi_rx_calc_ipi_tx_delay             0x00012ca5   Thumb Code   252  drv_dsi_rx.o(i.drv_dsi_rx_calc_ipi_tx_delay)
    drv_dsi_rx_enable_irq                    0x00012db1   Thumb Code    58  drv_dsi_rx.o(i.drv_dsi_rx_enable_irq)
    drv_dsi_rx_get_compression_en            0x00012e5d   Thumb Code    10  drv_dsi_rx.o(i.drv_dsi_rx_get_compression_en)
    drv_dsi_rx_get_ddi_crc_en                0x00012e6d   Thumb Code    10  drv_dsi_rx.o(i.drv_dsi_rx_get_ddi_crc_en)
    drv_dsi_rx_power_up                      0x00012e7d   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_power_up)
    drv_dsi_rx_set_check_crc                 0x00012e95   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_check_crc)
    drv_dsi_rx_set_ctrl_cfg                  0x00012eb1   Thumb Code    32  drv_dsi_rx.o(i.drv_dsi_rx_set_ctrl_cfg)
    drv_dsi_rx_set_ddi_cfg                   0x00012ed5   Thumb Code    10  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_cfg)
    drv_dsi_rx_set_ddi_crc_en                0x00012ee5   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_ddi_crc_en)
    drv_dsi_rx_set_inten                     0x00012f01   Thumb Code     8  drv_dsi_rx.o(i.drv_dsi_rx_set_inten)
    drv_dsi_rx_set_ipi_cfg                   0x00012f0d   Thumb Code    12  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_cfg)
    drv_dsi_rx_set_ipi_ycbcr_frmt            0x00012f1d   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_ipi_ycbcr_frmt)
    drv_dsi_rx_set_lane_swap                 0x00012f39   Thumb Code    16  drv_dsi_rx.o(i.drv_dsi_rx_set_lane_swap)
    drv_dsi_rx_set_resp_cnt                  0x00012f4d   Thumb Code    32  drv_dsi_rx.o(i.drv_dsi_rx_set_resp_cnt)
    drv_dsi_rx_set_tear_resp_en              0x00012f71   Thumb Code    24  drv_dsi_rx.o(i.drv_dsi_rx_set_tear_resp_en)
    drv_dsi_rx_set_up_phy                    0x00012f8d   Thumb Code   224  drv_dsi_rx.o(i.drv_dsi_rx_set_up_phy)
    drv_dsi_rx_shut_down                     0x0001308d   Thumb Code    14  drv_dsi_rx.o(i.drv_dsi_rx_shut_down)
    drv_dsi_tx_command_header                0x000130a5   Thumb Code    18  drv_dsi_tx.o(i.drv_dsi_tx_command_header)
    drv_dsi_tx_command_mode_cfg              0x000130bd   Thumb Code    82  drv_dsi_tx.o(i.drv_dsi_tx_command_mode_cfg)
    drv_dsi_tx_command_put_payload           0x00013115   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_command_put_payload)
    drv_dsi_tx_config_eotp                   0x00013121   Thumb Code    26  drv_dsi_tx.o(i.drv_dsi_tx_config_eotp)
    drv_dsi_tx_config_int                    0x00013141   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_config_int)
    drv_dsi_tx_dpi_lpcmd_time                0x0001314d   Thumb Code    10  drv_dsi_tx.o(i.drv_dsi_tx_dpi_lpcmd_time)
    drv_dsi_tx_dpi_mode                      0x0001315d   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_dpi_mode)
    drv_dsi_tx_dpi_polarity                  0x0001316d   Thumb Code    32  drv_dsi_tx.o(i.drv_dsi_tx_dpi_polarity)
    drv_dsi_tx_edpi_cmd_size                 0x00013191   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_edpi_cmd_size)
    drv_dsi_tx_get_cmd_status                0x0001319d   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_get_cmd_status)
    drv_dsi_tx_mode                          0x000131a9   Thumb Code     6  drv_dsi_tx.o(i.drv_dsi_tx_mode)
    drv_dsi_tx_phy_clock_lane_auto_lp        0x000131b5   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_auto_lp)
    drv_dsi_tx_phy_clock_lane_req_hs         0x000131d1   Thumb Code    26  drv_dsi_tx.o(i.drv_dsi_tx_phy_clock_lane_req_hs)
    drv_dsi_tx_phy_lane_mode                 0x000131f1   Thumb Code    12  drv_dsi_tx.o(i.drv_dsi_tx_phy_lane_mode)
    drv_dsi_tx_phy_status_ready              0x00013201   Thumb Code   100  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_ready)
    drv_dsi_tx_phy_status_stopstate          0x00013269   Thumb Code    62  drv_dsi_tx.o(i.drv_dsi_tx_phy_status_stopstate)
    drv_dsi_tx_phy_test_setup                0x000132ad   Thumb Code   314  drv_dsi_tx.o(i.drv_dsi_tx_phy_test_setup)
    drv_dsi_tx_phy_time_cfg                  0x000133fd   Thumb Code    28  drv_dsi_tx.o(i.drv_dsi_tx_phy_time_cfg)
    drv_dsi_tx_powerup                       0x0001341d   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_powerup)
    drv_dsi_tx_response_mode                 0x00013429   Thumb Code    30  drv_dsi_tx.o(i.drv_dsi_tx_response_mode)
    drv_dsi_tx_set_bta_ack                   0x0001344d   Thumb Code    24  drv_dsi_tx.o(i.drv_dsi_tx_set_bta_ack)
    drv_dsi_tx_set_esc_div                   0x00013469   Thumb Code    14  drv_dsi_tx.o(i.drv_dsi_tx_set_esc_div)
    drv_dsi_tx_set_int                       0x0001347d   Thumb Code    58  drv_dsi_tx.o(i.drv_dsi_tx_set_int)
    drv_dsi_tx_set_time_out_div              0x000134bd   Thumb Code    18  drv_dsi_tx.o(i.drv_dsi_tx_set_time_out_div)
    drv_dsi_tx_set_video_chunk               0x000134d5   Thumb Code    14  drv_dsi_tx.o(i.drv_dsi_tx_set_video_chunk)
    drv_dsi_tx_set_video_timing              0x000134e9   Thumb Code    30  drv_dsi_tx.o(i.drv_dsi_tx_set_video_timing)
    drv_dsi_tx_shutdown                      0x0001350d   Thumb Code     8  drv_dsi_tx.o(i.drv_dsi_tx_shutdown)
    drv_dsi_tx_timeout_cfg                   0x00013519   Thumb Code    38  drv_dsi_tx.o(i.drv_dsi_tx_timeout_cfg)
    drv_dsi_tx_video_mode_cfg                0x00013545   Thumb Code   226  drv_dsi_tx.o(i.drv_dsi_tx_video_mode_cfg)
    drv_efuse_enter_inactive                 0x0001362d   Thumb Code    54  drv_efuse.o(i.drv_efuse_enter_inactive)
    drv_efuse_int_enable                     0x00013663   Thumb Code    12  drv_efuse.o(i.drv_efuse_int_enable)
    drv_efuse_read                           0x0001366f   Thumb Code    58  drv_efuse.o(i.drv_efuse_read)
    drv_efuse_read_req                       0x000136a9   Thumb Code    24  drv_efuse.o(i.drv_efuse_read_req)
    drv_gpio_register_ap_reset_callback      0x000136e5   Thumb Code     6  drv_gpio.o(i.drv_gpio_register_ap_reset_callback)
    drv_gpio_register_callback               0x000136f1   Thumb Code    14  drv_gpio.o(i.drv_gpio_register_callback)
    drv_gpio_set_int                         0x00013705   Thumb Code    62  drv_gpio.o(i.drv_gpio_set_int)
    drv_gpio_set_ioe                         0x00013749   Thumb Code    26  drv_gpio.o(i.drv_gpio_set_ioe)
    drv_gpio_set_mode                        0x00013769   Thumb Code    16  drv_gpio.o(i.drv_gpio_set_mode)
    drv_lcdc_bcsa_config                     0x0001379d   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_bcsa_config)
    drv_lcdc_cfg_int_frame                   0x000137c5   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_cfg_int_frame)
    drv_lcdc_cmd_start                       0x00013809   Thumb Code    46  drv_lcdc.o(i.drv_lcdc_cmd_start)
    drv_lcdc_config_acc_command_mode         0x0001383d   Thumb Code    14  drv_lcdc.o(i.drv_lcdc_config_acc_command_mode)
    drv_lcdc_config_int                      0x00013851   Thumb Code    50  drv_lcdc.o(i.drv_lcdc_config_int)
    drv_lcdc_config_int_single               0x00013889   Thumb Code    34  drv_lcdc.o(i.drv_lcdc_config_int_single)
    drv_lcdc_config_overwrite_rgb            0x000138b1   Thumb Code    18  drv_lcdc.o(i.drv_lcdc_config_overwrite_rgb)
    drv_lcdc_config_src_parameter            0x000138c9   Thumb Code    72  drv_lcdc.o(i.drv_lcdc_config_src_parameter)
    drv_lcdc_crop_hact                       0x00013919   Thumb Code    10  drv_lcdc.o(i.drv_lcdc_crop_hact)
    drv_lcdc_ctrl_flow                       0x00013929   Thumb Code    50  drv_lcdc.o(i.drv_lcdc_ctrl_flow)
    drv_lcdc_dith_config                     0x00013961   Thumb Code    40  drv_lcdc.o(i.drv_lcdc_dith_config)
    drv_lcdc_edge_dect_config                0x00013991   Thumb Code    50  drv_lcdc.o(i.drv_lcdc_edge_dect_config)
    drv_lcdc_edge_enh_config                 0x000139cd   Thumb Code    86  drv_lcdc.o(i.drv_lcdc_edge_enh_config)
    drv_lcdc_enable_shadow_reg               0x00013a31   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_enable_shadow_reg)
    drv_lcdc_endianness_config               0x00013a55   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_endianness_config)
    drv_lcdc_fc_config                       0x00013a71   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_fc_config)
    drv_lcdc_fldc_config                     0x00013a91   Thumb Code    32  drv_lcdc.o(i.drv_lcdc_fldc_config)
    drv_lcdc_function_disable                0x00013ab5   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_function_disable)
    drv_lcdc_function_enable                 0x00013ad9   Thumb Code    30  drv_lcdc.o(i.drv_lcdc_function_enable)
    drv_lcdc_set_int                         0x00013afd   Thumb Code    54  drv_lcdc.o(i.drv_lcdc_set_int)
    drv_lcdc_set_prefetch                    0x00013b39   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_set_prefetch)
    drv_lcdc_set_tear_line                   0x00013b55   Thumb Code    24  drv_lcdc.o(i.drv_lcdc_set_tear_line)
    drv_lcdc_stop_display                    0x00013b71   Thumb Code    12  drv_lcdc.o(i.drv_lcdc_stop_display)
    drv_lcdc_vid_hw_start                    0x00013b81   Thumb Code    56  drv_lcdc.o(i.drv_lcdc_vid_hw_start)
    drv_lcdc_vintp_mode_config               0x00013bbd   Thumb Code    18  drv_lcdc.o(i.drv_lcdc_vintp_mode_config)
    drv_memc_clear_status                    0x00013bd5   Thumb Code    14  drv_memc.o(i.drv_memc_clear_status)
    drv_memc_enable_irq                      0x00013be9   Thumb Code    58  drv_memc.o(i.drv_memc_enable_irq)
    drv_memc_gen_a_tear_signal               0x00013c29   Thumb Code    12  drv_memc.o(i.drv_memc_gen_a_tear_signal)
    drv_memc_get_status                      0x00013c39   Thumb Code    20  drv_memc.o(i.drv_memc_get_status)
    drv_memc_get_tear_mode                   0x00013c51   Thumb Code    10  drv_memc.o(i.drv_memc_get_tear_mode)
    drv_memc_rate_transfer_sel               0x00013c61   Thumb Code    22  drv_memc.o(i.drv_memc_rate_transfer_sel)
    drv_memc_sel_vsync                       0x00013c7d   Thumb Code    16  drv_memc.o(i.drv_memc_sel_vsync)
    drv_memc_set_active_height               0x00013c91   Thumb Code    16  drv_memc.o(i.drv_memc_set_active_height)
    drv_memc_set_circ_mode_enable            0x00013ca9   Thumb Code    24  drv_memc.o(i.drv_memc_set_circ_mode_enable)
    drv_memc_set_data_mode                   0x00013cc5   Thumb Code    14  drv_memc.o(i.drv_memc_set_data_mode)
    drv_memc_set_double_buffer               0x00013cd9   Thumb Code    18  drv_memc.o(i.drv_memc_set_double_buffer)
    drv_memc_set_frame_drop_select           0x00013cf1   Thumb Code    24  drv_memc.o(i.drv_memc_set_frame_drop_select)
    drv_memc_set_fs_en_conditions            0x00013d0d   Thumb Code    18  drv_memc.o(i.drv_memc_set_fs_en_conditions)
    drv_memc_set_lcdc_st_conditions          0x00013d25   Thumb Code    20  drv_memc.o(i.drv_memc_set_lcdc_st_conditions)
    drv_memc_set_ltpo_mode                   0x00013d41   Thumb Code    28  drv_memc.o(i.drv_memc_set_ltpo_mode)
    drv_memc_set_ltpo_pu_thres               0x00013d61   Thumb Code    18  drv_memc.o(i.drv_memc_set_ltpo_pu_thres)
    drv_memc_set_tear_mode                   0x00013d79   Thumb Code    16  drv_memc.o(i.drv_memc_set_tear_mode)
    drv_memc_set_tear_waveform               0x00013d8d   Thumb Code    36  drv_memc.o(i.drv_memc_set_tear_waveform)
    drv_memc_set_vidc_sync_cnt               0x00013db9   Thumb Code    16  drv_memc.o(i.drv_memc_set_vidc_sync_cnt)
    drv_phy_test_clear                       0x00013dcd   Thumb Code    16  drv_phy_common.o(i.drv_phy_test_clear)
    drv_phy_test_lock                        0x00013ddd   Thumb Code    24  drv_phy_common.o(i.drv_phy_test_lock)
    drv_pwr_efuse_pd                         0x00013df5   Thumb Code    36  drv_pwr.o(i.drv_pwr_efuse_pd)
    drv_pwr_enter_deep_sleep_mode            0x00013e25   Thumb Code    60  drv_pwr.o(i.drv_pwr_enter_deep_sleep_mode)
    drv_pwr_enter_sleep_mode_ex              0x00013e71   Thumb Code    34  drv_pwr.o(i.drv_pwr_enter_sleep_mode_ex)
    drv_pwr_enter_stop_sleep_mode            0x00013ea5   Thumb Code   132  drv_pwr.o(i.drv_pwr_enter_stop_sleep_mode)
    drv_pwr_exit_sleep_mode                  0x00013f3d   Thumb Code    32  drv_pwr.o(i.drv_pwr_exit_sleep_mode)
    drv_pwr_get_power_ready_st               0x00013f65   Thumb Code    10  drv_pwr.o(i.drv_pwr_get_power_ready_st)
    drv_pwr_set_breath_screen_power_sel      0x00013f75   Thumb Code    34  drv_pwr.o(i.drv_pwr_set_breath_screen_power_sel)
    drv_pwr_set_digit_power_sel              0x00013f9d   Thumb Code    34  drv_pwr.o(i.drv_pwr_set_digit_power_sel)
    drv_pwr_set_pll_clk                      0x00013fc5   Thumb Code    30  drv_pwr.o(i.drv_pwr_set_pll_clk)
    drv_pwr_set_wakeup_type                  0x00013ff9   Thumb Code    40  drv_pwr.o(i.drv_pwr_set_wakeup_type)
    drv_pwr_write_lock                       0x00014025   Thumb Code    18  drv_pwr.o(i.drv_pwr_write_lock)
    drv_rxbr_clear_pkt_buffer                0x00014045   Thumb Code    12  drv_rxbr.o(i.drv_rxbr_clear_pkt_buffer)
    drv_rxbr_clear_status0                   0x00014055   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_clear_status0)
    drv_rxbr_enable_irq                      0x00014061   Thumb Code    90  drv_rxbr.o(i.drv_rxbr_enable_irq)
    drv_rxbr_frame_drop_cfg                  0x000140bd   Thumb Code    18  drv_rxbr.o(i.drv_rxbr_frame_drop_cfg)
    drv_rxbr_hline_rcv1_cfg                  0x00014109   Thumb Code    14  drv_rxbr.o(i.drv_rxbr_hline_rcv1_cfg)
    drv_rxbr_hline_rcv_cfg                   0x0001411d   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_hline_rcv_cfg)
    drv_rxbr_register_irq1_callback          0x0001412d   Thumb Code     6  drv_rxbr.o(i.drv_rxbr_register_irq1_callback)
    drv_rxbr_set_cmd_response                0x00014139   Thumb Code   320  drv_rxbr.o(i.drv_rxbr_set_cmd_response)
    drv_rxbr_set_color_format                0x0001427d   Thumb Code    24  drv_rxbr.o(i.drv_rxbr_set_color_format)
    drv_rxbr_set_filter_regs                 0x00014299   Thumb Code    32  drv_rxbr.o(i.drv_rxbr_set_filter_regs)
    drv_rxbr_set_inten                       0x000142bd   Thumb Code    22  drv_rxbr.o(i.drv_rxbr_set_inten)
    drv_rxbr_set_ltpo_drop_th                0x000142d9   Thumb Code    18  drv_rxbr.o(i.drv_rxbr_set_ltpo_drop_th)
    drv_rxbr_set_usr_cfg                     0x000142f1   Thumb Code    56  drv_rxbr.o(i.drv_rxbr_set_usr_cfg)
    drv_rxbr_set_usr_col                     0x00014331   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_set_usr_col)
    drv_rxbr_set_usr_row                     0x00014341   Thumb Code    10  drv_rxbr.o(i.drv_rxbr_set_usr_row)
    drv_se_init                              0x00014351   Thumb Code   106  drv_se.o(i.drv_se_init)
    drv_se_set_dsc                           0x000143c9   Thumb Code   162  drv_se.o(i.drv_se_set_dsc)
    drv_se_set_lcdc                          0x0001449d   Thumb Code    88  drv_se.o(i.drv_se_set_lcdc)
    drv_se_set_memc                          0x00014525   Thumb Code    96  drv_se.o(i.drv_se_set_memc)
    drv_se_set_rxbr                          0x000145b5   Thumb Code   158  drv_se.o(i.drv_se_set_rxbr)
    drv_se_set_vidc                          0x00014685   Thumb Code   122  drv_se.o(i.drv_se_set_vidc)
    drv_se_start_rx                          0x00014731   Thumb Code    16  drv_se.o(i.drv_se_start_rx)
    drv_spim_clear_int_status                0x00014745   Thumb Code     8  drv_spi_master.o(i.drv_spim_clear_int_status)
    drv_spim_disable_int                     0x00014751   Thumb Code    38  drv_spi_master.o(i.drv_spim_disable_int)
    drv_spim_set_inten                       0x00014781   Thumb Code    22  drv_spi_master.o(i.drv_spim_set_inten)
    drv_swire_enable                         0x0001479d   Thumb Code    24  drv_swire.o(i.drv_swire_enable)
    drv_swire_get_pulse_count                0x000147b9   Thumb Code     6  drv_swire.o(i.drv_swire_get_pulse_count)
    drv_swire_register_callback              0x000147c5   Thumb Code     6  drv_swire.o(i.drv_swire_register_callback)
    drv_swire_set_bit_time                   0x000147d1   Thumb Code    18  drv_swire.o(i.drv_swire_set_bit_time)
    drv_swire_set_int                        0x000147e9   Thumb Code    64  drv_swire.o(i.drv_swire_set_int)
    drv_swire_set_power_down                 0x00014831   Thumb Code    24  drv_swire.o(i.drv_swire_set_power_down)
    drv_swire_set_pulse_count                0x0001484d   Thumb Code     6  drv_swire.o(i.drv_swire_set_pulse_count)
    drv_swire_set_trig_mode                  0x00014859   Thumb Code    24  drv_swire.o(i.drv_swire_set_trig_mode)
    drv_sys_cfg_clear_all_int                0x00014875   Thumb Code     8  drv_sys_cfg.o(i.drv_sys_cfg_clear_all_int)
    drv_sys_cfg_clear_pending                0x00014881   Thumb Code    32  drv_sys_cfg.o(i.drv_sys_cfg_clear_pending)
    drv_sys_cfg_sel_ap_rst_trig              0x000148a9   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_sel_ap_rst_trig)
    drv_sys_cfg_sel_gpio_group               0x000148cd   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_sel_gpio_group)
    drv_sys_cfg_sel_int_trig                 0x000148f1   Thumb Code    32  drv_sys_cfg.o(i.drv_sys_cfg_sel_int_trig)
    drv_sys_cfg_sel_swire_timer              0x00014915   Thumb Code    18  drv_sys_cfg.o(i.drv_sys_cfg_sel_swire_timer)
    drv_sys_cfg_set_int                      0x0001492d   Thumb Code    30  drv_sys_cfg.o(i.drv_sys_cfg_set_int)
    drv_timer_enable                         0x0001496b   Thumb Code    32  drv_timer.o(i.drv_timer_enable)
    drv_timer_get_instance                   0x0001498d   Thumb Code    10  drv_timer.o(i.drv_timer_get_instance)
    drv_timer_register_callback              0x000149d9   Thumb Code    14  drv_timer.o(i.drv_timer_register_callback)
    drv_timer_set_compare_val                0x000149ed   Thumb Code    50  drv_timer.o(i.drv_timer_set_compare_val)
    drv_timer_set_int                        0x00014a2d   Thumb Code    68  drv_timer.o(i.drv_timer_set_int)
    drv_timer_set_prescaler                  0x00014a75   Thumb Code    36  drv_timer.o(i.drv_timer_set_prescaler)
    drv_timer_set_repeat                     0x00014a9d   Thumb Code    12  drv_timer.o(i.drv_timer_set_repeat)
    drv_tx_phy_test_enter                    0x00014aad   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_enter)
    drv_tx_phy_test_exit                     0x00014acd   Thumb Code    28  drv_dsi_tx.o(i.drv_tx_phy_test_exit)
    drv_tx_phy_test_write_code               0x00014aed   Thumb Code    34  drv_dsi_tx.o(i.drv_tx_phy_test_write_code)
    drv_uart_abort_recv                      0x00014b15   Thumb Code    46  drv_uart.o(i.drv_uart_abort_recv)
    drv_uart_abort_send                      0x00014b49   Thumb Code    46  drv_uart.o(i.drv_uart_abort_send)
    drv_uart_config_int                      0x00014b7d   Thumb Code    20  drv_uart.o(i.drv_uart_config_int)
    drv_uart_enable_int                      0x00014ba9   Thumb Code    84  drv_uart.o(i.drv_uart_enable_int)
    drv_uart_get_instance                    0x00014c05   Thumb Code    36  drv_uart.o(i.drv_uart_get_instance)
    drv_uart_init                            0x00014c2d   Thumb Code   206  drv_uart.o(i.drv_uart_init)
    drv_uart_reset_rx_fifo                   0x00014d39   Thumb Code    28  drv_uart.o(i.drv_uart_reset_rx_fifo)
    drv_uart_reset_tx_fifo                   0x00014d55   Thumb Code    28  drv_uart.o(i.drv_uart_reset_tx_fifo)
    drv_uart_send_blocking                   0x00014d71   Thumb Code    26  drv_uart.o(i.drv_uart_send_blocking)
    drv_uart_set_baud_rate                   0x00014d8b   Thumb Code    84  drv_uart.o(i.drv_uart_set_baud_rate)
    drv_uart_trans_create_handle             0x00014de1   Thumb Code    72  drv_uart.o(i.drv_uart_trans_create_handle)
    drv_vidc_clear_irq                       0x00014e2d   Thumb Code    10  drv_vidc.o(i.drv_vidc_clear_irq)
    drv_vidc_enable                          0x00014e3d   Thumb Code    26  drv_vidc.o(i.drv_vidc_enable)
    drv_vidc_enable_irq                      0x00014e5d   Thumb Code    58  drv_vidc.o(i.drv_vidc_enable_irq)
    drv_vidc_get_int_source                  0x00014e9d   Thumb Code    40  drv_vidc.o(i.drv_vidc_get_int_source)
    drv_vidc_get_irq_status                  0x00014ec9   Thumb Code    20  drv_vidc.o(i.drv_vidc_get_irq_status)
    drv_vidc_init_module_enable              0x00014ee1   Thumb Code    36  drv_vidc.o(i.drv_vidc_init_module_enable)
    drv_vidc_register_callback               0x00014f0d   Thumb Code     6  drv_vidc.o(i.drv_vidc_register_callback)
    drv_vidc_reset                           0x00014f19   Thumb Code     8  drv_vidc.o(i.drv_vidc_reset)
    drv_vidc_set_circ_mode_enable            0x00014f25   Thumb Code    24  drv_vidc.o(i.drv_vidc_set_circ_mode_enable)
    drv_vidc_set_dither_config               0x00014f41   Thumb Code    50  drv_vidc.o(i.drv_vidc_set_dither_config)
    drv_vidc_set_dst_parameter               0x00014f79   Thumb Code    86  drv_vidc.o(i.drv_vidc_set_dst_parameter)
    drv_vidc_set_honly_hcoef0                0x00014fd5   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_honly_hcoef0)
    drv_vidc_set_honly_hinitb                0x00014fe1   Thumb Code    38  drv_vidc.o(i.drv_vidc_set_honly_hinitb)
    drv_vidc_set_honly_hinitr                0x0001500d   Thumb Code    42  drv_vidc.o(i.drv_vidc_set_honly_hinitr)
    drv_vidc_set_irqen                       0x0001503d   Thumb Code    22  drv_vidc.o(i.drv_vidc_set_irqen)
    drv_vidc_set_mirror                      0x00015059   Thumb Code    16  drv_vidc.o(i.drv_vidc_set_mirror)
    drv_vidc_set_pentile_swap                0x0001506d   Thumb Code    20  drv_vidc.o(i.drv_vidc_set_pentile_swap)
    drv_vidc_set_pu_ctrl                     0x00015089   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_pu_ctrl)
    drv_vidc_set_rotation                    0x00015095   Thumb Code    18  drv_vidc.o(i.drv_vidc_set_rotation)
    drv_vidc_set_scld_hcoef0                 0x000150ad   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_hcoef0)
    drv_vidc_set_scld_hcoef1                 0x000150b9   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_hcoef1)
    drv_vidc_set_scld_step                   0x000150c5   Thumb Code    14  drv_vidc.o(i.drv_vidc_set_scld_step)
    drv_vidc_set_scld_vcoef0                 0x000150d9   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_vcoef0)
    drv_vidc_set_scld_vcoef1                 0x000150e5   Thumb Code     6  drv_vidc.o(i.drv_vidc_set_scld_vcoef1)
    drv_vidc_set_src_parameter               0x000150f1   Thumb Code    28  drv_vidc.o(i.drv_vidc_set_src_parameter)
    drv_vidc_set_vintp_config                0x00015111   Thumb Code    52  drv_vidc.o(i.drv_vidc_set_vintp_config)
    drv_wdg_clear_counter                    0x00015149   Thumb Code    12  drv_wdg.o(i.drv_wdg_clear_counter)
    drv_wdg_set_int                          0x00015179   Thumb Code    48  drv_wdg.o(i.drv_wdg_set_int)
    fputc                                    0x000151ad   Thumb Code    42  tau_log.o(i.fputc)
    hal_dsi_rx_ctrl_create_handle            0x00015221   Thumb Code    60  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_create_handle)
    hal_dsi_rx_ctrl_dcs_async_handler        0x00015261   Thumb Code    60  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_dcs_async_handler)
    hal_dsi_rx_ctrl_deinit                   0x000152a1   Thumb Code   132  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_deinit)
    hal_dsi_rx_ctrl_init                     0x00015335   Thumb Code   158  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_init)
    hal_dsi_rx_ctrl_pre_init_pps             0x00015acd   Thumb Code    50  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_pre_init_pps)
    hal_dsi_rx_ctrl_set_auto_ack             0x00015b05   Thumb Code   148  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_set_auto_ack)
    hal_dsi_rx_ctrl_start                    0x00015be5   Thumb Code    42  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_start)
    hal_dsi_rx_ctrl_stop                     0x00015c15   Thumb Code    42  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_stop)
    hal_dsi_rx_ctrl_toggle_resolution        0x00015c45   Thumb Code    28  hal_dsi_rx_ctrl.o(i.hal_dsi_rx_ctrl_toggle_resolution)
    hal_dsi_tx_ctrl_create_handle            0x00015ee1   Thumb Code    48  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_create_handle)
    hal_dsi_tx_ctrl_deinit                   0x00015f19   Thumb Code   102  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_deinit)
    hal_dsi_tx_ctrl_gen_a_tear_signal        0x00015f8d   Thumb Code    34  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_gen_a_tear_signal)
    hal_dsi_tx_ctrl_init                     0x00015fb1   Thumb Code   110  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_init)
    hal_dsi_tx_ctrl_set_overwrite_rgb        0x0001603d   Thumb Code     8  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_overwrite_rgb)
    hal_dsi_tx_ctrl_set_tear_mode            0x00016045   Thumb Code    10  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_set_tear_mode)
    hal_dsi_tx_ctrl_start                    0x00016051   Thumb Code   134  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_start)
    hal_dsi_tx_ctrl_stop                     0x000160e1   Thumb Code    52  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_stop)
    hal_dsi_tx_ctrl_write_array_cmd          0x00016119   Thumb Code   238  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_array_cmd)
    hal_dsi_tx_ctrl_write_cmd                0x0001620d   Thumb Code   202  hal_dsi_tx_ctrl.o(i.hal_dsi_tx_ctrl_write_cmd)
    hal_gpio_config_pad                      0x000168b9   Thumb Code    58  hal_gpio.o(i.hal_gpio_config_pad)
    hal_gpio_ctrl_eint                       0x000168f5   Thumb Code    18  hal_gpio.o(i.hal_gpio_ctrl_eint)
    hal_gpio_init_eint                       0x0001690d   Thumb Code    58  hal_gpio.o(i.hal_gpio_init_eint)
    hal_gpio_init_input                      0x0001694d   Thumb Code    22  hal_gpio.o(i.hal_gpio_init_input)
    hal_gpio_init_output                     0x00016963   Thumb Code    28  hal_gpio.o(i.hal_gpio_init_output)
    hal_gpio_reg_eint_cb                     0x00016981   Thumb Code    22  hal_gpio.o(i.hal_gpio_reg_eint_cb)
    hal_gpio_set_ap_reset_int                0x0001699d   Thumb Code    76  hal_gpio.o(i.hal_gpio_set_ap_reset_int)
    hal_gpio_set_mode                        0x000169ed   Thumb Code    92  hal_gpio.o(i.hal_gpio_set_mode)
    hal_gpio_set_output_data                 0x00016a4d   Thumb Code     8  hal_gpio.o(i.hal_gpio_set_output_data)
    hal_internal_sync_get_hight_performan_mode 0x00016a55   Thumb Code    10  hal_internal_vsync.o(i.hal_internal_sync_get_hight_performan_mode)
    hal_internal_sync_input_resolution_change 0x00016a65   Thumb Code   326  hal_internal_vsync.o(i.hal_internal_sync_input_resolution_change)
    hal_internal_sync_register_lcdc_cb       0x00016c11   Thumb Code     8  hal_internal_vsync.o(i.hal_internal_sync_register_lcdc_cb)
    hal_internal_vsync_deinit                0x00016c1d   Thumb Code    22  hal_internal_vsync.o(i.hal_internal_vsync_deinit)
    hal_internal_vsync_get_rx_state          0x00016c3d   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_rx_state)
    hal_internal_vsync_get_sync_line         0x00016c49   Thumb Code    16  hal_internal_vsync.o(i.hal_internal_vsync_get_sync_line)
    hal_internal_vsync_get_tx_state          0x00016c5d   Thumb Code     6  hal_internal_vsync.o(i.hal_internal_vsync_get_tx_state)
    hal_internal_vsync_init_rx               0x00016c69   Thumb Code   206  hal_internal_vsync.o(i.hal_internal_vsync_init_rx)
    hal_internal_vsync_init_tx               0x00016d51   Thumb Code   194  hal_internal_vsync.o(i.hal_internal_vsync_init_tx)
    hal_internal_vsync_set_rx_state          0x00016e19   Thumb Code    28  hal_internal_vsync.o(i.hal_internal_vsync_set_rx_state)
    hal_internal_vsync_set_tear_mode         0x00016e39   Thumb Code   306  hal_internal_vsync.o(i.hal_internal_vsync_set_tear_mode)
    hal_internal_vsync_set_tx_state          0x00016f7d   Thumb Code    78  hal_internal_vsync.o(i.hal_internal_vsync_set_tx_state)
    hal_intl_dcs_init_sw_fltr                0x00016fd5   Thumb Code    90  hal_internal_dcs.o(i.hal_intl_dcs_init_sw_fltr)
    hal_intl_dcs_set_auto_hw_filter          0x00017689   Thumb Code   130  hal_internal_dcs.o(i.hal_intl_dcs_set_auto_hw_filter)
    hal_intl_fb_cal_fb_info                  0x00017741   Thumb Code   738  hal_internal_fb.o(i.hal_intl_fb_cal_fb_info)
    hal_intl_fb_get_memc_flow_mode           0x00017be5   Thumb Code     6  hal_internal_fb.o(i.hal_intl_fb_get_memc_flow_mode)
    hal_intl_fb_get_rx_fb_info               0x00017bf1   Thumb Code    12  hal_internal_fb.o(i.hal_intl_fb_get_rx_fb_info)
    hal_intl_fb_get_tx_fb_info               0x00017c01   Thumb Code    12  hal_internal_fb.o(i.hal_intl_fb_get_tx_fb_info)
    hal_intl_fb_get_user_flow                0x00017c11   Thumb Code     6  hal_internal_fb.o(i.hal_intl_fb_get_user_flow)
    hal_intl_svs_deinit_rx                   0x00017c1d   Thumb Code    32  hal_internal_svs.o(i.hal_intl_svs_deinit_rx)
    hal_intl_svs_deinit_tx                   0x00017c45   Thumb Code    10  hal_internal_svs.o(i.hal_intl_svs_deinit_tx)
    hal_intl_svs_handle                      0x00017c55   Thumb Code    24  hal_internal_svs.o(i.hal_intl_svs_handle)
    hal_intl_svs_init_rx                     0x00017c79   Thumb Code   120  hal_internal_svs.o(i.hal_intl_svs_init_rx)
    hal_intl_svs_init_tx                     0x00017cf9   Thumb Code    16  hal_internal_svs.o(i.hal_intl_svs_init_tx)
    hal_intl_svs_set_rx_vtt                  0x00017d0d   Thumb Code     6  hal_internal_svs.o(i.hal_intl_svs_set_rx_vtt)
    hal_intl_svs_update_rxbr_clk             0x00017d19   Thumb Code    52  hal_internal_svs.o(i.hal_intl_svs_update_rxbr_clk)
    hal_lcdc_displayproc_config              0x00017d61   Thumb Code    94  hal_dsi_tx_ctrl.o(i.hal_lcdc_displayproc_config)
    hal_lcdc_postproc_config                 0x00017e81   Thumb Code   276  hal_dsi_tx_ctrl.o(i.hal_lcdc_postproc_config)
    hal_lcdc_upscaler_config                 0x00018009   Thumb Code   202  hal_dsi_tx_ctrl.o(i.hal_lcdc_upscaler_config)
    hal_nonshadow_func_update                0x000180e9   Thumb Code   180  hal_dsi_tx_ctrl.o(i.hal_nonshadow_func_update)
    hal_pwr_enter_deep_sleep_mode            0x000181a5   Thumb Code    42  hal_pwr.o(i.hal_pwr_enter_deep_sleep_mode)
    hal_pwr_enter_normal_sleep_mode          0x000181cf   Thumb Code     8  hal_pwr.o(i.hal_pwr_enter_normal_sleep_mode)
    hal_pwr_enter_stop_sleep_mode            0x000181d9   Thumb Code    88  hal_pwr.o(i.hal_pwr_enter_stop_sleep_mode)
    hal_pwr_exit_sleep_mode                  0x0001823d   Thumb Code    10  hal_pwr.o(i.hal_pwr_exit_sleep_mode)
    hal_pwr_get_vcc_power_ready              0x00018247   Thumb Code     8  hal_pwr.o(i.hal_pwr_get_vcc_power_ready)
    hal_pwr_set_main_power                   0x0001824f   Thumb Code     8  hal_pwr.o(i.hal_pwr_set_main_power)
    hal_pwr_set_sleep_mode_power             0x00018257   Thumb Code     8  hal_pwr.o(i.hal_pwr_set_sleep_mode_power)
    hal_pwr_set_stop_sleep_wakeup_pin        0x00018261   Thumb Code    86  hal_pwr.o(i.hal_pwr_set_stop_sleep_wakeup_pin)
    hal_swire_deinit                         0x000182c5   Thumb Code    60  hal_swire.o(i.hal_swire_deinit)
    hal_swire_enable                         0x00018305   Thumb Code    86  hal_swire.o(i.hal_swire_enable)
    hal_swire_init                           0x00018361   Thumb Code    74  hal_swire.o(i.hal_swire_init)
    hal_swire_set_pulse                      0x000183b9   Thumb Code    32  hal_swire.o(i.hal_swire_set_pulse)
    hal_swire_set_timer                      0x000183dd   Thumb Code    60  hal_swire.o(i.hal_swire_set_timer)
    hal_system_init                          0x0001841d   Thumb Code   192  hal_system.o(i.hal_system_init)
    hal_system_updata_sysclk                 0x00018501   Thumb Code    60  hal_system.o(i.hal_system_updata_sysclk)
    hal_timer_deinit                         0x00018551   Thumb Code    48  hal_timer.o(i.hal_timer_deinit)
    hal_timer_init                           0x00018581   Thumb Code    28  hal_timer.o(i.hal_timer_init)
    hal_timer_set_repeat                     0x0001859d   Thumb Code     8  hal_timer.o(i.hal_timer_set_repeat)
    hal_timer_start                          0x000185a5   Thumb Code    48  hal_timer.o(i.hal_timer_start)
    hal_timer_stop                           0x000185d5   Thumb Code    40  hal_timer.o(i.hal_timer_stop)
    hal_uart_init                            0x0001862d   Thumb Code   134  hal_uart.o(i.hal_uart_init)
    hal_uart_send_blocking                   0x000186c1   Thumb Code    24  hal_uart.o(i.hal_uart_send_blocking)
    hal_vsync_func_update                    0x000186dd   Thumb Code    18  hal_dsi_tx_ctrl.o(i.hal_vsync_func_update)
    hal_vsync_reset_lcdc_scaler              0x000186f5   Thumb Code   206  hal_internal_vsync.o(i.hal_vsync_reset_lcdc_scaler)
    main                                     0x000187d5   Thumb Code    32  main.o(i.main)
    s8_demo                                  0x00018b4d   Thumb Code    48  s8_demo.o(i.s8_demo)
    tau_log_init                             0x000191ed   Thumb Code    48  tau_log.o(i.tau_log_init)
    tau_log_printf                           0x00019221   Thumb Code   116  tau_log.o(i.tau_log_printf)
    tau_log_push_log                         0x000192a5   Thumb Code   118  tau_log.o(i.tau_log_push_log)
    panel_init_code                          0x00019548   Data        7815  s8_demo.o(.constdata)
    Region$$Table$$Base                      0x0001b6c8   Number         0  anon$$obj.o(Region$$Table)
    Region$$Table$$Limit                     0x0001b6e8   Number         0  anon$$obj.o(Region$$Table)
    s_swire_pwm_counter                      0x0007000d   Data           1  s8_demo.o(.data)
    t_pps                                    0x0007000e   Data         128  s8_demo.o(.data)
    sg_uart0_tx_handle                       0x00070120   Data           4  hal_uart.o(.data)
    sg_uart0_rx_handle                       0x00070124   Data           4  hal_uart.o(.data)
    sg_uart1_tx_handle                       0x00070128   Data           4  hal_uart.o(.data)
    sg_uart1_rx_handle                       0x0007012c   Data           4  hal_uart.o(.data)
    g_sof_gen_te_func                        0x0007013c   Data           4  hal_internal_vsync.o(.data)
    hal_internal_vsync_handle_callback       0x00070140   Data           4  hal_internal_vsync.o(.data)
    hal_internal_disp_end_handle_callback    0x00070144   Data           4  hal_internal_vsync.o(.data)
    g_systick_cb_func                        0x00070170   Data           4  drv_common.o(.data)
    g_system_clock                           0x00070174   Data           4  drv_common.o(.data)
    g_system_delay_step                      0x00070178   Data           1  drv_common.o(.data)
    dma_req_map                              0x0007027c   Data         144  drv_dma.o(.data)
    drv_i2c_table                            0x00070370   Data          36  drv_i2c.o(.data)
    g_int_rxbr_irq0_cb_func                  0x0007039c   Data           4  drv_rxbr.o(.data)
    g_int_rxbr_irq1_cb_func                  0x000703a0   Data           4  drv_rxbr.o(.data)
    g_int_vidc_cb_func                       0x000703a4   Data           4  drv_vidc.o(.data)
    __stdout                                 0x000703a8   Data           4  stdout.o(.data)
    g_vsync_handle                           0x00070634   Data          40  hal_internal_vsync.o(.bss)
    sg_pro_motion_handle                     0x0007065c   Data          28  hal_internal_vsync.o(.bss)
    g_dcs_execute_table                      0x00070678   Data        2048  hal_internal_dcs.o(.bss)
    g_rx_fb_info                             0x00070f78   Data          68  hal_internal_fb.o(.bss)
    g_packet_fifo                            0x00071050   Data        4204  dcs_packet_fifo.o(.bss)
    __stack_limit                            0x00072120   Data           0  startup_armcm0.o(STACK)
    __initial_sp                             0x00073120   Data           0  startup_armcm0.o(STACK)



==============================================================================

Memory Map of the image

  Image Entry point : 0x000100c1

  Load Region LR_IROM2 (Base: 0x00010000, Size: 0x0000ba94, Max: 0x00010000, ABSOLUTE, COMPRESSED[0x0000b848])

    Execution Region ER_IROM2 (Exec base: 0x00010000, Load base: 0x00010000, Size: 0x0000b6e8, Max: 0x00010000, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00010000   0x00010000   0x000000c0   Data   RO          538    RESET               startup_armcm0.o
    0x000100c0   0x000100c0   0x00000000   Code   RO         2670  * .ARM.Collect$$$$00000000  mc_p.l(entry.o)
    0x000100c0   0x000100c0   0x00000004   Code   RO         2976    .ARM.Collect$$$$00000001  mc_p.l(entry2.o)
    0x000100c4   0x000100c4   0x00000004   Code   RO         2979    .ARM.Collect$$$$00000004  mc_p.l(entry5.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         2981    .ARM.Collect$$$$00000008  mc_p.l(entry7b.o)
    0x000100c8   0x000100c8   0x00000000   Code   RO         2983    .ARM.Collect$$$$0000000A  mc_p.l(entry8b.o)
    0x000100c8   0x000100c8   0x00000008   Code   RO         2984    .ARM.Collect$$$$0000000B  mc_p.l(entry9a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         2986    .ARM.Collect$$$$0000000D  mc_p.l(entry10a.o)
    0x000100d0   0x000100d0   0x00000000   Code   RO         2988    .ARM.Collect$$$$0000000F  mc_p.l(entry11a.o)
    0x000100d0   0x000100d0   0x00000004   Code   RO         2977    .ARM.Collect$$$$00002712  mc_p.l(entry2.o)
    0x000100d4   0x000100d4   0x00000078   Code   RO          539    .text               startup_armcm0.o
    0x0001014c   0x0001014c   0x0000002c   Code   RO         2673    .text               mc_p.l(uidiv.o)
    0x00010178   0x00010178   0x00000028   Code   RO         2675    .text               mc_p.l(idiv.o)
    0x000101a0   0x000101a0   0x00000024   Code   RO         2677    .text               mc_p.l(memcpya.o)
    0x000101c4   0x000101c4   0x00000024   Code   RO         2679    .text               mc_p.l(memseta.o)
    0x000101e8   0x000101e8   0x0000000e   Code   RO         2681    .text               mc_p.l(strlen.o)
    0x000101f6   0x000101f6   0x000000b2   Code   RO         2946    .text               mf_p.l(fadd.o)
    0x000102a8   0x000102a8   0x0000007a   Code   RO         2948    .text               mf_p.l(fmul.o)
    0x00010322   0x00010322   0x0000007c   Code   RO         2950    .text               mf_p.l(fdiv.o)
    0x0001039e   0x0001039e   0x00000018   Code   RO         2952    .text               mf_p.l(fscalb.o)
    0x000103b6   0x000103b6   0x00000002   PAD
    0x000103b8   0x000103b8   0x00000164   Code   RO         2954    .text               mf_p.l(dadd.o)
    0x0001051c   0x0001051c   0x000000d0   Code   RO         2956    .text               mf_p.l(dmul.o)
    0x000105ec   0x000105ec   0x000000f0   Code   RO         2958    .text               mf_p.l(ddiv.o)
    0x000106dc   0x000106dc   0x0000000e   Code   RO         2960    .text               mf_p.l(ffltui.o)
    0x000106ea   0x000106ea   0x00000002   PAD
    0x000106ec   0x000106ec   0x0000001c   Code   RO         2962    .text               mf_p.l(dfltui.o)
    0x00010708   0x00010708   0x00000028   Code   RO         2964    .text               mf_p.l(ffixui.o)
    0x00010730   0x00010730   0x0000003c   Code   RO         2966    .text               mf_p.l(dfixui.o)
    0x0001076c   0x0001076c   0x00000028   Code   RO         2968    .text               mf_p.l(f2d.o)
    0x00010794   0x00010794   0x00000038   Code   RO         2970    .text               mf_p.l(d2f.o)
    0x000107cc   0x000107cc   0x00000014   Code   RO         2972    .text               mf_p.l(cfcmple.o)
    0x000107e0   0x000107e0   0x00000014   Code   RO         2974    .text               mf_p.l(cfrcmple.o)
    0x000107f4   0x000107f4   0x00000060   Code   RO         2991    .text               mc_p.l(uldiv.o)
    0x00010854   0x00010854   0x00000020   Code   RO         2993    .text               mc_p.l(llshl.o)
    0x00010874   0x00010874   0x00000022   Code   RO         2995    .text               mc_p.l(llushr.o)
    0x00010896   0x00010896   0x00000026   Code   RO         2997    .text               mc_p.l(llsshr.o)
    0x000108bc   0x000108bc   0x00000000   Code   RO         2999    .text               mc_p.l(iusefp.o)
    0x000108bc   0x000108bc   0x00000082   Code   RO         3000    .text               mf_p.l(fepilogue.o)
    0x0001093e   0x0001093e   0x000000be   Code   RO         3002    .text               mf_p.l(depilogue.o)
    0x000109fc   0x000109fc   0x00000040   Code   RO         3006    .text               mf_p.l(dfixul.o)
    0x00010a3c   0x00010a3c   0x00000028   Code   RO         3008    .text               mf_p.l(cdrcmple.o)
    0x00010a64   0x00010a64   0x00000024   Code   RO         3010    .text               mc_p.l(init.o)
    0x00010a88   0x00010a88   0x00000056   Code   RO         3020    .text               mc_p.l(__dczerorl2.o)
    0x00010ade   0x00010ade   0x00000002   PAD
    0x00010ae0   0x00010ae0   0x0000001c   Code   RO         1663    i.AP_NRESET_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010afc   0x00010afc   0x0000005c   Code   RO         1588    i.DMA_IRQn_Handler  CVWL668.lib(drv_dma.o)
    0x00010b58   0x00010b58   0x0000000a   Code   RO         1664    i.EXTI_INT0_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010b62   0x00010b62   0x0000000a   Code   RO         1665    i.EXTI_INT1_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010b6c   0x00010b6c   0x0000000a   Code   RO         1666    i.EXTI_INT2_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010b76   0x00010b76   0x0000000a   Code   RO         1667    i.EXTI_INT3_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010b80   0x00010b80   0x0000000a   Code   RO         1668    i.EXTI_INT4_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010b8a   0x00010b8a   0x0000000a   Code   RO         1669    i.EXTI_INT5_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010b94   0x00010b94   0x0000000a   Code   RO         1670    i.EXTI_INT6_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010b9e   0x00010b9e   0x0000000a   Code   RO         1671    i.EXTI_INT7_IRQn_Handler  CVWL668.lib(drv_gpio.o)
    0x00010ba8   0x00010ba8   0x00000048   Code   RO         1523    i.HardFault_Handler  CVWL668.lib(drv_common.o)
    0x00010bf0   0x00010bf0   0x0000000c   Code   RO         1984    i.I2C0_IRQn_Handler  CVWL668.lib(drv_i2c.o)
    0x00010bfc   0x00010bfc   0x0000000c   Code   RO         1985    i.I2C1_IRQn_Handler  CVWL668.lib(drv_i2c.o)
    0x00010c08   0x00010c08   0x0000000c   Code   RO         1986    i.I2C2_IRQn_Handler  CVWL668.lib(drv_i2c.o)
    0x00010c14   0x00010c14   0x00000100   Code   RO         1368    i.LCDC_IRQn_Handler  CVWL668.lib(hal_internal_vsync.o)
    0x00010d14   0x00010d14   0x0000009a   Code   RO         2352    i.MEMC_IRQn_Handler  CVWL668.lib(drv_memc.o)
    0x00010dae   0x00010dae   0x00000002   PAD
    0x00010db0   0x00010db0   0x000000b8   Code   RO         2158    i.MIPI_TX_IRQn_Handler  CVWL668.lib(drv_dsi_tx.o)
    0x00010e68   0x00010e68   0x00000048   Code   RO         1147    i.SPIM_IRQn_Handler  CVWL668.lib(hal_spi_master.o)
    0x00010eb0   0x00010eb0   0x00000030   Code   RO         1843    i.SWIRE_IRQn_Handler  CVWL668.lib(drv_swire.o)
    0x00010ee0   0x00010ee0   0x00000018   Code   RO         1524    i.SysTick_Handler   CVWL668.lib(drv_common.o)
    0x00010ef8   0x00010ef8   0x0000000a   Code   RO         1886    i.TIMER0_IRQn_Handler  CVWL668.lib(drv_timer.o)
    0x00010f02   0x00010f02   0x0000000a   Code   RO         1887    i.TIMER1_IRQn_Handler  CVWL668.lib(drv_timer.o)
    0x00010f0c   0x00010f0c   0x0000000a   Code   RO         1888    i.TIMER2_IRQn_Handler  CVWL668.lib(drv_timer.o)
    0x00010f16   0x00010f16   0x0000000a   Code   RO         1889    i.TIMER3_IRQn_Handler  CVWL668.lib(drv_timer.o)
    0x00010f20   0x00010f20   0x0000001c   Code   RO         2507    i.VIDC_IRQn_Handler  CVWL668.lib(drv_vidc.o)
    0x00010f3c   0x00010f3c   0x0000001c   Code   RO         2418    i.VPRE1_IRQn_Handler  CVWL668.lib(drv_rxbr.o)
    0x00010f58   0x00010f58   0x0000006c   Code   RO         1434    i.VPRE_IRQn_Handler  CVWL668.lib(hal_internal_dcs.o)
    0x00010fc4   0x00010fc4   0x00000038   Code   RO         1919    i.WDG_IRQn_Handler  CVWL668.lib(drv_wdg.o)
    0x00010ffc   0x00010ffc   0x00000002   Code   RO         3015    i.__scatterload_null  mc_p.l(handlers.o)
    0x00010ffe   0x00010ffe   0x00000002   PAD
    0x00011000   0x00011000   0x0000001c   Data   RO         1531    .ARM.__at_0x11000   CVWL668.lib(drv_common.o)
    0x0001101c   0x0001101c   0x00000010   Data   RO         1324    .ARM.__at_0x1101C   CVWL668.lib(tau_log.o)
    0x0001102c   0x0001102c   0x00000016   Data   RO         1016    .ARM.__at_0x1102C   CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00011042   0x00011042   0x00000002   PAD
    0x00011044   0x00011044   0x00000364   Code   RO         2097    i.MIPI_RX_IRQn_Handler  CVWL668.lib(drv_dsi_rx.o)
    0x000113a8   0x000113a8   0x00000180   Code   RO         2592    i.UART_IRQn_Handler  CVWL668.lib(drv_uart.o)
    0x00011528   0x00011528   0x00000020   Code   RO         2918    i.__0printf         mc_p.l(printfa.o)
    0x00011548   0x00011548   0x00000024   Code   RO         2924    i.__0vsprintf       mc_p.l(printfa.o)
    0x0001156c   0x0001156c   0x0000002e   Code   RO         3004    i.__ARM_clz         mf_p.l(depilogue.o)
    0x0001159a   0x0001159a   0x0000001a   Code   RO          963    i.__ARM_common_switch8  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x000115b4   0x000115b4   0x00000020   Code   RO         2419    i.__NVIC_DisableIRQ  CVWL668.lib(drv_rxbr.o)
    0x000115d4   0x000115d4   0x00000018   Code   RO         2420    i.__NVIC_EnableIRQ  CVWL668.lib(drv_rxbr.o)
    0x000115ec   0x000115ec   0x0000000e   Code   RO         3014    i.__scatterload_copy  mc_p.l(handlers.o)
    0x000115fa   0x000115fa   0x0000000e   Code   RO         3016    i.__scatterload_zeroinit  mc_p.l(handlers.o)
    0x00011608   0x00011608   0x00000174   Code   RO         2925    i._fp_digits        mc_p.l(printfa.o)
    0x0001177c   0x0001177c   0x000006ec   Code   RO         2926    i._printf_core      mc_p.l(printfa.o)
    0x00011e68   0x00011e68   0x00000020   Code   RO         2927    i._printf_post_padding  mc_p.l(printfa.o)
    0x00011e88   0x00011e88   0x0000002c   Code   RO         2928    i._printf_pre_padding  mc_p.l(printfa.o)
    0x00011eb4   0x00011eb4   0x0000000a   Code   RO         2930    i._sputc            mc_p.l(printfa.o)
    0x00011ebe   0x00011ebe   0x00000002   PAD
    0x00011ec0   0x00011ec0   0x000000b0   Code   RO          322    i.ap_dcs_set_backlight  s8_demo.o
    0x00011f70   0x00011f70   0x00000006   Code   RO          323    i.ap_dcs_set_display_off  s8_demo.o
    0x00011f76   0x00011f76   0x00000002   PAD
    0x00011f78   0x00011f78   0x0000003c   Code   RO          324    i.ap_dcs_set_display_on  s8_demo.o
    0x00011fb4   0x00011fb4   0x00000050   Code   RO          325    i.ap_dcs_set_enter_sleep_mode  s8_demo.o
    0x00012004   0x00012004   0x00000064   Code   RO          326    i.ap_dcs_set_exit_sleep_mode  s8_demo.o
    0x00012068   0x00012068   0x00000054   Code   RO          329    i.ap_rstn_pull_high_cb  s8_demo.o
    0x000120bc   0x000120bc   0x00000080   Code   RO          330    i.ap_set_framerate  s8_demo.o
    0x0001213c   0x0001213c   0x00000084   Code   RO          331    i.ap_update_pps_9E  s8_demo.o
    0x000121c0   0x000121c0   0x00000068   Code   RO          332    i.app_display_init  s8_demo.o
    0x00012228   0x00012228   0x00000020   Code   RO          333    i.app_gpio_init     s8_demo.o
    0x00012248   0x00012248   0x00000048   Code   RO          334    i.app_init_panel    s8_demo.o
    0x00012290   0x00012290   0x000000e8   Code   RO          335    i.app_mipi_rx_init  s8_demo.o
    0x00012378   0x00012378   0x000000c0   Code   RO          337    i.app_mipi_tx_init  s8_demo.o
    0x00012438   0x00012438   0x0000006c   Code   RO          338    i.app_mipi_tx_start  s8_demo.o
    0x000124a4   0x000124a4   0x0000008c   Code   RO          339    i.app_set_dcs_hw_ack  s8_demo.o
    0x00012530   0x00012530   0x0000004c   Code   RO          340    i.app_system_process  s8_demo.o
    0x0001257c   0x0001257c   0x00000048   Code   RO          341    i.app_system_resume  s8_demo.o
    0x000125c4   0x000125c4   0x00000124   Code   RO          342    i.app_system_suspend  s8_demo.o
    0x000126e8   0x000126e8   0x0000002e   Code   RO          343    i.app_tx_panel_reset  s8_demo.o
    0x00012716   0x00012716   0x00000002   PAD
    0x00012718   0x00012718   0x00000018   Code   RO          518    i.board_Init        board.o
    0x00012730   0x00012730   0x000000c8   Code   RO         2667    i.ceil              m_ps.l(ceil.o)
    0x000127f8   0x000127f8   0x0000002c   Code   RO         1369    i.check_mipi_rx_tx_video_info  CVWL668.lib(hal_internal_vsync.o)
    0x00012824   0x00012824   0x00000088   Code   RO         1435    i.check_pkt_buf_rev  CVWL668.lib(hal_internal_dcs.o)
    0x000128ac   0x000128ac   0x00000058   Code   RO         2063    i.dcs_packet_fifo_alloc  CVWL668.lib(dcs_packet_fifo.o)
    0x00012904   0x00012904   0x00000018   Code   RO         2064    i.dcs_packet_fifo_init  CVWL668.lib(dcs_packet_fifo.o)
    0x0001291c   0x0001291c   0x00000044   Code   RO         2065    i.dcs_packet_free_fifo_header  CVWL668.lib(dcs_packet_fifo.o)
    0x00012960   0x00012960   0x00000024   Code   RO         2066    i.dcs_packet_get_fifo_header  CVWL668.lib(dcs_packet_fifo.o)
    0x00012984   0x00012984   0x00000018   Code   RO         1311    i.delayMs           CVWL668.lib(tau_delay.o)
    0x0001299c   0x0001299c   0x0000002c   Code   RO         1312    i.delayUs           CVWL668.lib(tau_delay.o)
    0x000129c8   0x000129c8   0x00000008   Code   RO         1529    i.drv_common_system_init  CVWL668.lib(drv_common.o)
    0x000129d0   0x000129d0   0x0000003c   Code   RO         1548    i.drv_crgu_enable_clock  CVWL668.lib(drv_crgu.o)
    0x00012a0c   0x00012a0c   0x00000068   Code   RO         1551    i.drv_crgu_get_rxbr_clk  CVWL668.lib(drv_crgu.o)
    0x00012a74   0x00012a74   0x00000010   Code   RO         1554    i.drv_crgu_reset_modules  CVWL668.lib(drv_crgu.o)
    0x00012a84   0x00012a84   0x00000028   Code   RO         1555    i.drv_crgu_set_ahb_clk  CVWL668.lib(drv_crgu.o)
    0x00012aac   0x00012aac   0x00000010   Code   RO         1556    i.drv_crgu_set_clock_div  CVWL668.lib(drv_crgu.o)
    0x00012abc   0x00012abc   0x0000003c   Code   RO         1558    i.drv_crgu_set_dpi_clk  CVWL668.lib(drv_crgu.o)
    0x00012af8   0x00012af8   0x00000038   Code   RO         1559    i.drv_crgu_set_dsc_clk  CVWL668.lib(drv_crgu.o)
    0x00012b30   0x00012b30   0x00000028   Code   RO         1560    i.drv_crgu_set_fb_clk  CVWL668.lib(drv_crgu.o)
    0x00012b58   0x00012b58   0x00000028   Code   RO         1561    i.drv_crgu_set_lcdc_clk  CVWL668.lib(drv_crgu.o)
    0x00012b80   0x00012b80   0x00000018   Code   RO         1562    i.drv_crgu_set_reset  CVWL668.lib(drv_crgu.o)
    0x00012b98   0x00012b98   0x00000028   Code   RO         1563    i.drv_crgu_set_rxbr_clk  CVWL668.lib(drv_crgu.o)
    0x00012bc0   0x00012bc0   0x00000028   Code   RO         1564    i.drv_crgu_set_vidc_clk  CVWL668.lib(drv_crgu.o)
    0x00012be8   0x00012be8   0x00000018   Code   RO         1590    i.drv_dma_clear_status  CVWL668.lib(drv_dma.o)
    0x00012c00   0x00012c00   0x00000014   Code   RO         1596    i.drv_dma_get_int_source  CVWL668.lib(drv_dma.o)
    0x00012c14   0x00012c14   0x0000001c   Code   RO         1651    i.drv_dsc_dec_disable  CVWL668.lib(drv_dsc_dec.o)
    0x00012c30   0x00012c30   0x00000038   Code   RO         1652    i.drv_dsc_dec_enable  CVWL668.lib(drv_dsc_dec.o)
    0x00012c68   0x00012c68   0x00000020   Code   RO         1653    i.drv_dsc_dec_get_nslc  CVWL668.lib(drv_dsc_dec.o)
    0x00012c88   0x00012c88   0x0000001c   Code   RO         1654    i.drv_dsc_dec_set_irqen  CVWL668.lib(drv_dsc_dec.o)
    0x00012ca4   0x00012ca4   0x0000010c   Code   RO         2098    i.drv_dsi_rx_calc_ipi_tx_delay  CVWL668.lib(drv_dsi_rx.o)
    0x00012db0   0x00012db0   0x00000040   Code   RO         2099    i.drv_dsi_rx_enable_irq  CVWL668.lib(drv_dsi_rx.o)
    0x00012df0   0x00012df0   0x00000050   Code   RO         2101    i.drv_dsi_rx_get_color_bpp  CVWL668.lib(drv_dsi_rx.o)
    0x00012e40   0x00012e40   0x0000001c   Code   RO         2102    i.drv_dsi_rx_get_color_pcc  CVWL668.lib(drv_dsi_rx.o)
    0x00012e5c   0x00012e5c   0x00000010   Code   RO         2103    i.drv_dsi_rx_get_compression_en  CVWL668.lib(drv_dsi_rx.o)
    0x00012e6c   0x00012e6c   0x00000010   Code   RO         2104    i.drv_dsi_rx_get_ddi_crc_en  CVWL668.lib(drv_dsi_rx.o)
    0x00012e7c   0x00012e7c   0x00000018   Code   RO         2109    i.drv_dsi_rx_power_up  CVWL668.lib(drv_dsi_rx.o)
    0x00012e94   0x00012e94   0x0000001c   Code   RO         2110    i.drv_dsi_rx_set_check_crc  CVWL668.lib(drv_dsi_rx.o)
    0x00012eb0   0x00012eb0   0x00000024   Code   RO         2111    i.drv_dsi_rx_set_ctrl_cfg  CVWL668.lib(drv_dsi_rx.o)
    0x00012ed4   0x00012ed4   0x00000010   Code   RO         2112    i.drv_dsi_rx_set_ddi_cfg  CVWL668.lib(drv_dsi_rx.o)
    0x00012ee4   0x00012ee4   0x0000001c   Code   RO         2113    i.drv_dsi_rx_set_ddi_crc_en  CVWL668.lib(drv_dsi_rx.o)
    0x00012f00   0x00012f00   0x0000000c   Code   RO         2116    i.drv_dsi_rx_set_inten  CVWL668.lib(drv_dsi_rx.o)
    0x00012f0c   0x00012f0c   0x00000010   Code   RO         2117    i.drv_dsi_rx_set_ipi_cfg  CVWL668.lib(drv_dsi_rx.o)
    0x00012f1c   0x00012f1c   0x0000001c   Code   RO         2119    i.drv_dsi_rx_set_ipi_ycbcr_frmt  CVWL668.lib(drv_dsi_rx.o)
    0x00012f38   0x00012f38   0x00000014   Code   RO         2120    i.drv_dsi_rx_set_lane_swap  CVWL668.lib(drv_dsi_rx.o)
    0x00012f4c   0x00012f4c   0x00000024   Code   RO         2121    i.drv_dsi_rx_set_resp_cnt  CVWL668.lib(drv_dsi_rx.o)
    0x00012f70   0x00012f70   0x0000001c   Code   RO         2122    i.drv_dsi_rx_set_tear_resp_en  CVWL668.lib(drv_dsi_rx.o)
    0x00012f8c   0x00012f8c   0x00000100   Code   RO         2123    i.drv_dsi_rx_set_up_phy  CVWL668.lib(drv_dsi_rx.o)
    0x0001308c   0x0001308c   0x00000018   Code   RO         2124    i.drv_dsi_rx_shut_down  CVWL668.lib(drv_dsi_rx.o)
    0x000130a4   0x000130a4   0x00000018   Code   RO         2160    i.drv_dsi_tx_command_header  CVWL668.lib(drv_dsi_tx.o)
    0x000130bc   0x000130bc   0x00000058   Code   RO         2161    i.drv_dsi_tx_command_mode_cfg  CVWL668.lib(drv_dsi_tx.o)
    0x00013114   0x00013114   0x0000000c   Code   RO         2162    i.drv_dsi_tx_command_put_payload  CVWL668.lib(drv_dsi_tx.o)
    0x00013120   0x00013120   0x00000020   Code   RO         2163    i.drv_dsi_tx_config_eotp  CVWL668.lib(drv_dsi_tx.o)
    0x00013140   0x00013140   0x0000000c   Code   RO         2164    i.drv_dsi_tx_config_int  CVWL668.lib(drv_dsi_tx.o)
    0x0001314c   0x0001314c   0x00000010   Code   RO         2165    i.drv_dsi_tx_dpi_lpcmd_time  CVWL668.lib(drv_dsi_tx.o)
    0x0001315c   0x0001315c   0x00000010   Code   RO         2166    i.drv_dsi_tx_dpi_mode  CVWL668.lib(drv_dsi_tx.o)
    0x0001316c   0x0001316c   0x00000024   Code   RO         2167    i.drv_dsi_tx_dpi_polarity  CVWL668.lib(drv_dsi_tx.o)
    0x00013190   0x00013190   0x0000000c   Code   RO         2168    i.drv_dsi_tx_edpi_cmd_size  CVWL668.lib(drv_dsi_tx.o)
    0x0001319c   0x0001319c   0x0000000c   Code   RO         2170    i.drv_dsi_tx_get_cmd_status  CVWL668.lib(drv_dsi_tx.o)
    0x000131a8   0x000131a8   0x0000000c   Code   RO         2172    i.drv_dsi_tx_mode   CVWL668.lib(drv_dsi_tx.o)
    0x000131b4   0x000131b4   0x0000001c   Code   RO         2173    i.drv_dsi_tx_phy_clock_lane_auto_lp  CVWL668.lib(drv_dsi_tx.o)
    0x000131d0   0x000131d0   0x00000020   Code   RO         2174    i.drv_dsi_tx_phy_clock_lane_req_hs  CVWL668.lib(drv_dsi_tx.o)
    0x000131f0   0x000131f0   0x00000010   Code   RO         2176    i.drv_dsi_tx_phy_lane_mode  CVWL668.lib(drv_dsi_tx.o)
    0x00013200   0x00013200   0x00000068   Code   RO         2179    i.drv_dsi_tx_phy_status_ready  CVWL668.lib(drv_dsi_tx.o)
    0x00013268   0x00013268   0x00000044   Code   RO         2180    i.drv_dsi_tx_phy_status_stopstate  CVWL668.lib(drv_dsi_tx.o)
    0x000132ac   0x000132ac   0x00000150   Code   RO         2182    i.drv_dsi_tx_phy_test_setup  CVWL668.lib(drv_dsi_tx.o)
    0x000133fc   0x000133fc   0x00000020   Code   RO         2183    i.drv_dsi_tx_phy_time_cfg  CVWL668.lib(drv_dsi_tx.o)
    0x0001341c   0x0001341c   0x0000000c   Code   RO         2187    i.drv_dsi_tx_powerup  CVWL668.lib(drv_dsi_tx.o)
    0x00013428   0x00013428   0x00000024   Code   RO         2188    i.drv_dsi_tx_response_mode  CVWL668.lib(drv_dsi_tx.o)
    0x0001344c   0x0001344c   0x0000001c   Code   RO         2191    i.drv_dsi_tx_set_bta_ack  CVWL668.lib(drv_dsi_tx.o)
    0x00013468   0x00013468   0x00000014   Code   RO         2192    i.drv_dsi_tx_set_esc_div  CVWL668.lib(drv_dsi_tx.o)
    0x0001347c   0x0001347c   0x00000040   Code   RO         2193    i.drv_dsi_tx_set_int  CVWL668.lib(drv_dsi_tx.o)
    0x000134bc   0x000134bc   0x00000018   Code   RO         2194    i.drv_dsi_tx_set_time_out_div  CVWL668.lib(drv_dsi_tx.o)
    0x000134d4   0x000134d4   0x00000014   Code   RO         2195    i.drv_dsi_tx_set_video_chunk  CVWL668.lib(drv_dsi_tx.o)
    0x000134e8   0x000134e8   0x00000024   Code   RO         2196    i.drv_dsi_tx_set_video_timing  CVWL668.lib(drv_dsi_tx.o)
    0x0001350c   0x0001350c   0x0000000c   Code   RO         2198    i.drv_dsi_tx_shutdown  CVWL668.lib(drv_dsi_tx.o)
    0x00013518   0x00013518   0x0000002c   Code   RO         2199    i.drv_dsi_tx_timeout_cfg  CVWL668.lib(drv_dsi_tx.o)
    0x00013544   0x00013544   0x000000e8   Code   RO         2202    i.drv_dsi_tx_video_mode_cfg  CVWL668.lib(drv_dsi_tx.o)
    0x0001362c   0x0001362c   0x00000036   Code   RO         2637    i.drv_efuse_enter_inactive  CVWL668.lib(drv_efuse.o)
    0x00013662   0x00013662   0x0000000c   Code   RO         2640    i.drv_efuse_int_enable  CVWL668.lib(drv_efuse.o)
    0x0001366e   0x0001366e   0x0000003a   Code   RO         2641    i.drv_efuse_read    CVWL668.lib(drv_efuse.o)
    0x000136a8   0x000136a8   0x00000018   Code   RO         2642    i.drv_efuse_read_req  CVWL668.lib(drv_efuse.o)
    0x000136c0   0x000136c0   0x00000024   Code   RO         1674    i.drv_gpio_handle_int  CVWL668.lib(drv_gpio.o)
    0x000136e4   0x000136e4   0x0000000c   Code   RO         1675    i.drv_gpio_register_ap_reset_callback  CVWL668.lib(drv_gpio.o)
    0x000136f0   0x000136f0   0x00000014   Code   RO         1676    i.drv_gpio_register_callback  CVWL668.lib(drv_gpio.o)
    0x00013704   0x00013704   0x00000044   Code   RO         1678    i.drv_gpio_set_int  CVWL668.lib(drv_gpio.o)
    0x00013748   0x00013748   0x00000020   Code   RO         1679    i.drv_gpio_set_ioe  CVWL668.lib(drv_gpio.o)
    0x00013768   0x00013768   0x00000014   Code   RO         1680    i.drv_gpio_set_mode  CVWL668.lib(drv_gpio.o)
    0x0001377c   0x0001377c   0x00000020   Code   RO         1073    i.drv_gpio_set_output_data  CVWL668.lib(hal_gpio.o)
    0x0001379c   0x0001379c   0x00000028   Code   RO         2264    i.drv_lcdc_bcsa_config  CVWL668.lib(drv_lcdc.o)
    0x000137c4   0x000137c4   0x0000002c   Code   RO         2265    i.drv_lcdc_cfg_int_frame  CVWL668.lib(drv_lcdc.o)
    0x000137f0   0x000137f0   0x00000018   Code   RO         2266    i.drv_lcdc_clear_int  CVWL668.lib(drv_lcdc.o)
    0x00013808   0x00013808   0x00000034   Code   RO         2268    i.drv_lcdc_cmd_start  CVWL668.lib(drv_lcdc.o)
    0x0001383c   0x0001383c   0x00000014   Code   RO         2269    i.drv_lcdc_config_acc_command_mode  CVWL668.lib(drv_lcdc.o)
    0x00013850   0x00013850   0x00000038   Code   RO         2270    i.drv_lcdc_config_int  CVWL668.lib(drv_lcdc.o)
    0x00013888   0x00013888   0x00000028   Code   RO         2271    i.drv_lcdc_config_int_single  CVWL668.lib(drv_lcdc.o)
    0x000138b0   0x000138b0   0x00000018   Code   RO         2272    i.drv_lcdc_config_overwrite_rgb  CVWL668.lib(drv_lcdc.o)
    0x000138c8   0x000138c8   0x00000050   Code   RO         2273    i.drv_lcdc_config_src_parameter  CVWL668.lib(drv_lcdc.o)
    0x00013918   0x00013918   0x00000010   Code   RO         2274    i.drv_lcdc_crop_hact  CVWL668.lib(drv_lcdc.o)
    0x00013928   0x00013928   0x00000038   Code   RO         2275    i.drv_lcdc_ctrl_flow  CVWL668.lib(drv_lcdc.o)
    0x00013960   0x00013960   0x00000030   Code   RO         2276    i.drv_lcdc_dith_config  CVWL668.lib(drv_lcdc.o)
    0x00013990   0x00013990   0x0000003c   Code   RO         2278    i.drv_lcdc_edge_dect_config  CVWL668.lib(drv_lcdc.o)
    0x000139cc   0x000139cc   0x00000064   Code   RO         2279    i.drv_lcdc_edge_enh_config  CVWL668.lib(drv_lcdc.o)
    0x00013a30   0x00013a30   0x00000024   Code   RO         2280    i.drv_lcdc_enable_shadow_reg  CVWL668.lib(drv_lcdc.o)
    0x00013a54   0x00013a54   0x0000001c   Code   RO         2281    i.drv_lcdc_endianness_config  CVWL668.lib(drv_lcdc.o)
    0x00013a70   0x00013a70   0x00000020   Code   RO         2282    i.drv_lcdc_fc_config  CVWL668.lib(drv_lcdc.o)
    0x00013a90   0x00013a90   0x00000024   Code   RO         2284    i.drv_lcdc_fldc_config  CVWL668.lib(drv_lcdc.o)
    0x00013ab4   0x00013ab4   0x00000024   Code   RO         2285    i.drv_lcdc_function_disable  CVWL668.lib(drv_lcdc.o)
    0x00013ad8   0x00013ad8   0x00000024   Code   RO         2286    i.drv_lcdc_function_enable  CVWL668.lib(drv_lcdc.o)
    0x00013afc   0x00013afc   0x0000003c   Code   RO         2297    i.drv_lcdc_set_int  CVWL668.lib(drv_lcdc.o)
    0x00013b38   0x00013b38   0x0000001c   Code   RO         2298    i.drv_lcdc_set_prefetch  CVWL668.lib(drv_lcdc.o)
    0x00013b54   0x00013b54   0x0000001c   Code   RO         2299    i.drv_lcdc_set_tear_line  CVWL668.lib(drv_lcdc.o)
    0x00013b70   0x00013b70   0x00000010   Code   RO         2301    i.drv_lcdc_stop_display  CVWL668.lib(drv_lcdc.o)
    0x00013b80   0x00013b80   0x0000003c   Code   RO         2303    i.drv_lcdc_vid_hw_start  CVWL668.lib(drv_lcdc.o)
    0x00013bbc   0x00013bbc   0x00000018   Code   RO         2305    i.drv_lcdc_vintp_mode_config  CVWL668.lib(drv_lcdc.o)
    0x00013bd4   0x00013bd4   0x00000014   Code   RO         2353    i.drv_memc_clear_status  CVWL668.lib(drv_memc.o)
    0x00013be8   0x00013be8   0x00000040   Code   RO         2354    i.drv_memc_enable_irq  CVWL668.lib(drv_memc.o)
    0x00013c28   0x00013c28   0x00000010   Code   RO         2355    i.drv_memc_gen_a_tear_signal  CVWL668.lib(drv_memc.o)
    0x00013c38   0x00013c38   0x00000018   Code   RO         2356    i.drv_memc_get_status  CVWL668.lib(drv_memc.o)
    0x00013c50   0x00013c50   0x00000010   Code   RO         2357    i.drv_memc_get_tear_mode  CVWL668.lib(drv_memc.o)
    0x00013c60   0x00013c60   0x0000001c   Code   RO         2358    i.drv_memc_rate_transfer_sel  CVWL668.lib(drv_memc.o)
    0x00013c7c   0x00013c7c   0x00000014   Code   RO         2359    i.drv_memc_sel_vsync  CVWL668.lib(drv_memc.o)
    0x00013c90   0x00013c90   0x00000018   Code   RO         2360    i.drv_memc_set_active_height  CVWL668.lib(drv_memc.o)
    0x00013ca8   0x00013ca8   0x0000001c   Code   RO         2361    i.drv_memc_set_circ_mode_enable  CVWL668.lib(drv_memc.o)
    0x00013cc4   0x00013cc4   0x00000014   Code   RO         2362    i.drv_memc_set_data_mode  CVWL668.lib(drv_memc.o)
    0x00013cd8   0x00013cd8   0x00000018   Code   RO         2365    i.drv_memc_set_double_buffer  CVWL668.lib(drv_memc.o)
    0x00013cf0   0x00013cf0   0x0000001c   Code   RO         2369    i.drv_memc_set_frame_drop_select  CVWL668.lib(drv_memc.o)
    0x00013d0c   0x00013d0c   0x00000018   Code   RO         2370    i.drv_memc_set_fs_en_conditions  CVWL668.lib(drv_memc.o)
    0x00013d24   0x00013d24   0x0000001c   Code   RO         2372    i.drv_memc_set_lcdc_st_conditions  CVWL668.lib(drv_memc.o)
    0x00013d40   0x00013d40   0x00000020   Code   RO         2373    i.drv_memc_set_ltpo_mode  CVWL668.lib(drv_memc.o)
    0x00013d60   0x00013d60   0x00000018   Code   RO         2374    i.drv_memc_set_ltpo_pu_thres  CVWL668.lib(drv_memc.o)
    0x00013d78   0x00013d78   0x00000014   Code   RO         2378    i.drv_memc_set_tear_mode  CVWL668.lib(drv_memc.o)
    0x00013d8c   0x00013d8c   0x0000002c   Code   RO         2379    i.drv_memc_set_tear_waveform  CVWL668.lib(drv_memc.o)
    0x00013db8   0x00013db8   0x00000014   Code   RO         2381    i.drv_memc_set_vidc_sync_cnt  CVWL668.lib(drv_memc.o)
    0x00013dcc   0x00013dcc   0x00000010   Code   RO         2660    i.drv_phy_test_clear  CVWL668.lib(drv_phy_common.o)
    0x00013ddc   0x00013ddc   0x00000018   Code   RO         2661    i.drv_phy_test_lock  CVWL668.lib(drv_phy_common.o)
    0x00013df4   0x00013df4   0x00000030   Code   RO         1710    i.drv_pwr_efuse_pd  CVWL668.lib(drv_pwr.o)
    0x00013e24   0x00013e24   0x0000004c   Code   RO         1712    i.drv_pwr_enter_deep_sleep_mode  CVWL668.lib(drv_pwr.o)
    0x00013e70   0x00013e70   0x00000034   Code   RO         1714    i.drv_pwr_enter_sleep_mode_ex  CVWL668.lib(drv_pwr.o)
    0x00013ea4   0x00013ea4   0x00000098   Code   RO         1715    i.drv_pwr_enter_stop_sleep_mode  CVWL668.lib(drv_pwr.o)
    0x00013f3c   0x00013f3c   0x00000028   Code   RO         1716    i.drv_pwr_exit_sleep_mode  CVWL668.lib(drv_pwr.o)
    0x00013f64   0x00013f64   0x00000010   Code   RO         1719    i.drv_pwr_get_power_ready_st  CVWL668.lib(drv_pwr.o)
    0x00013f74   0x00013f74   0x00000028   Code   RO         1751    i.drv_pwr_set_breath_screen_power_sel  CVWL668.lib(drv_pwr.o)
    0x00013f9c   0x00013f9c   0x00000028   Code   RO         1752    i.drv_pwr_set_digit_power_sel  CVWL668.lib(drv_pwr.o)
    0x00013fc4   0x00013fc4   0x00000034   Code   RO         1755    i.drv_pwr_set_pll_clk  CVWL668.lib(drv_pwr.o)
    0x00013ff8   0x00013ff8   0x0000002c   Code   RO         1759    i.drv_pwr_set_wakeup_type  CVWL668.lib(drv_pwr.o)
    0x00014024   0x00014024   0x00000020   Code   RO         1762    i.drv_pwr_write_lock  CVWL668.lib(drv_pwr.o)
    0x00014044   0x00014044   0x00000010   Code   RO         2421    i.drv_rxbr_clear_pkt_buffer  CVWL668.lib(drv_rxbr.o)
    0x00014054   0x00014054   0x0000000c   Code   RO         2422    i.drv_rxbr_clear_status0  CVWL668.lib(drv_rxbr.o)
    0x00014060   0x00014060   0x0000005a   Code   RO         2425    i.drv_rxbr_enable_irq  CVWL668.lib(drv_rxbr.o)
    0x000140ba   0x000140ba   0x00000002   PAD
    0x000140bc   0x000140bc   0x0000001c   Code   RO         2426    i.drv_rxbr_frame_drop_cfg  CVWL668.lib(drv_rxbr.o)
    0x000140d8   0x000140d8   0x00000018   Code   RO         1370    i.drv_rxbr_get_int_source  CVWL668.lib(hal_internal_vsync.o)
    0x000140f0   0x000140f0   0x00000018   Code   RO         1436    i.drv_rxbr_get_status0  CVWL668.lib(hal_internal_dcs.o)
    0x00014108   0x00014108   0x00000014   Code   RO         2436    i.drv_rxbr_hline_rcv1_cfg  CVWL668.lib(drv_rxbr.o)
    0x0001411c   0x0001411c   0x00000010   Code   RO         2437    i.drv_rxbr_hline_rcv_cfg  CVWL668.lib(drv_rxbr.o)
    0x0001412c   0x0001412c   0x0000000c   Code   RO         2439    i.drv_rxbr_register_irq1_callback  CVWL668.lib(drv_rxbr.o)
    0x00014138   0x00014138   0x00000144   Code   RO         2443    i.drv_rxbr_set_cmd_response  CVWL668.lib(drv_rxbr.o)
    0x0001427c   0x0001427c   0x0000001c   Code   RO         2445    i.drv_rxbr_set_color_format  CVWL668.lib(drv_rxbr.o)
    0x00014298   0x00014298   0x00000024   Code   RO         2448    i.drv_rxbr_set_filter_regs  CVWL668.lib(drv_rxbr.o)
    0x000142bc   0x000142bc   0x0000001c   Code   RO         2449    i.drv_rxbr_set_inten  CVWL668.lib(drv_rxbr.o)
    0x000142d8   0x000142d8   0x00000018   Code   RO         2450    i.drv_rxbr_set_ltpo_drop_th  CVWL668.lib(drv_rxbr.o)
    0x000142f0   0x000142f0   0x00000040   Code   RO         2454    i.drv_rxbr_set_usr_cfg  CVWL668.lib(drv_rxbr.o)
    0x00014330   0x00014330   0x00000010   Code   RO         2455    i.drv_rxbr_set_usr_col  CVWL668.lib(drv_rxbr.o)
    0x00014340   0x00014340   0x00000010   Code   RO         2456    i.drv_rxbr_set_usr_row  CVWL668.lib(drv_rxbr.o)
    0x00014350   0x00014350   0x00000078   Code   RO         2078    i.drv_se_init       CVWL668.lib(drv_se.o)
    0x000143c8   0x000143c8   0x000000d4   Code   RO         2079    i.drv_se_set_dsc    CVWL668.lib(drv_se.o)
    0x0001449c   0x0001449c   0x00000088   Code   RO         2080    i.drv_se_set_lcdc   CVWL668.lib(drv_se.o)
    0x00014524   0x00014524   0x00000090   Code   RO         2081    i.drv_se_set_memc   CVWL668.lib(drv_se.o)
    0x000145b4   0x000145b4   0x000000d0   Code   RO         2082    i.drv_se_set_rxbr   CVWL668.lib(drv_se.o)
    0x00014684   0x00014684   0x000000ac   Code   RO         2083    i.drv_se_set_vidc   CVWL668.lib(drv_se.o)
    0x00014730   0x00014730   0x00000014   Code   RO         2084    i.drv_se_start_rx   CVWL668.lib(drv_se.o)
    0x00014744   0x00014744   0x0000000c   Code   RO         1825    i.drv_spim_clear_int_status  CVWL668.lib(drv_spi_master.o)
    0x00014750   0x00014750   0x00000030   Code   RO         1826    i.drv_spim_disable_int  CVWL668.lib(drv_spi_master.o)
    0x00014780   0x00014780   0x0000001c   Code   RO         1830    i.drv_spim_set_inten  CVWL668.lib(drv_spi_master.o)
    0x0001479c   0x0001479c   0x0000001c   Code   RO         1844    i.drv_swire_enable  CVWL668.lib(drv_swire.o)
    0x000147b8   0x000147b8   0x0000000c   Code   RO         1845    i.drv_swire_get_pulse_count  CVWL668.lib(drv_swire.o)
    0x000147c4   0x000147c4   0x0000000c   Code   RO         1846    i.drv_swire_register_callback  CVWL668.lib(drv_swire.o)
    0x000147d0   0x000147d0   0x00000018   Code   RO         1847    i.drv_swire_set_bit_time  CVWL668.lib(drv_swire.o)
    0x000147e8   0x000147e8   0x00000048   Code   RO         1848    i.drv_swire_set_int  CVWL668.lib(drv_swire.o)
    0x00014830   0x00014830   0x0000001c   Code   RO         1849    i.drv_swire_set_power_down  CVWL668.lib(drv_swire.o)
    0x0001484c   0x0001484c   0x0000000c   Code   RO         1850    i.drv_swire_set_pulse_count  CVWL668.lib(drv_swire.o)
    0x00014858   0x00014858   0x0000001c   Code   RO         1851    i.drv_swire_set_trig_mode  CVWL668.lib(drv_swire.o)
    0x00014874   0x00014874   0x0000000c   Code   RO         1866    i.drv_sys_cfg_clear_all_int  CVWL668.lib(drv_sys_cfg.o)
    0x00014880   0x00014880   0x00000028   Code   RO         1867    i.drv_sys_cfg_clear_pending  CVWL668.lib(drv_sys_cfg.o)
    0x000148a8   0x000148a8   0x00000024   Code   RO         1868    i.drv_sys_cfg_sel_ap_rst_trig  CVWL668.lib(drv_sys_cfg.o)
    0x000148cc   0x000148cc   0x00000024   Code   RO         1870    i.drv_sys_cfg_sel_gpio_group  CVWL668.lib(drv_sys_cfg.o)
    0x000148f0   0x000148f0   0x00000024   Code   RO         1871    i.drv_sys_cfg_sel_int_trig  CVWL668.lib(drv_sys_cfg.o)
    0x00014914   0x00014914   0x00000018   Code   RO         1872    i.drv_sys_cfg_sel_swire_timer  CVWL668.lib(drv_sys_cfg.o)
    0x0001492c   0x0001492c   0x00000024   Code   RO         1873    i.drv_sys_cfg_set_int  CVWL668.lib(drv_sys_cfg.o)
    0x00014950   0x00014950   0x0000001a   Code   RO         1890    i.drv_timer_clear_status_flags  CVWL668.lib(drv_timer.o)
    0x0001496a   0x0001496a   0x00000020   Code   RO         1891    i.drv_timer_enable  CVWL668.lib(drv_timer.o)
    0x0001498a   0x0001498a   0x00000002   PAD
    0x0001498c   0x0001498c   0x00000010   Code   RO         1892    i.drv_timer_get_instance  CVWL668.lib(drv_timer.o)
    0x0001499c   0x0001499c   0x0000003c   Code   RO         1894    i.drv_timer_handle_interrupt  CVWL668.lib(drv_timer.o)
    0x000149d8   0x000149d8   0x00000014   Code   RO         1895    i.drv_timer_register_callback  CVWL668.lib(drv_timer.o)
    0x000149ec   0x000149ec   0x00000040   Code   RO         1896    i.drv_timer_set_compare_val  CVWL668.lib(drv_timer.o)
    0x00014a2c   0x00014a2c   0x00000048   Code   RO         1897    i.drv_timer_set_int  CVWL668.lib(drv_timer.o)
    0x00014a74   0x00014a74   0x00000028   Code   RO         1898    i.drv_timer_set_prescaler  CVWL668.lib(drv_timer.o)
    0x00014a9c   0x00014a9c   0x00000010   Code   RO         1899    i.drv_timer_set_repeat  CVWL668.lib(drv_timer.o)
    0x00014aac   0x00014aac   0x00000020   Code   RO         2204    i.drv_tx_phy_test_enter  CVWL668.lib(drv_dsi_tx.o)
    0x00014acc   0x00014acc   0x00000020   Code   RO         2205    i.drv_tx_phy_test_exit  CVWL668.lib(drv_dsi_tx.o)
    0x00014aec   0x00014aec   0x00000028   Code   RO         2208    i.drv_tx_phy_test_write_code  CVWL668.lib(drv_dsi_tx.o)
    0x00014b14   0x00014b14   0x00000034   Code   RO         2593    i.drv_uart_abort_recv  CVWL668.lib(drv_uart.o)
    0x00014b48   0x00014b48   0x00000034   Code   RO         2594    i.drv_uart_abort_send  CVWL668.lib(drv_uart.o)
    0x00014b7c   0x00014b7c   0x00000014   Code   RO         2595    i.drv_uart_config_int  CVWL668.lib(drv_uart.o)
    0x00014b90   0x00014b90   0x00000018   Code   RO         2597    i.drv_uart_enable_clk  CVWL668.lib(drv_uart.o)
    0x00014ba8   0x00014ba8   0x0000005c   Code   RO         2598    i.drv_uart_enable_int  CVWL668.lib(drv_uart.o)
    0x00014c04   0x00014c04   0x00000028   Code   RO         2600    i.drv_uart_get_instance  CVWL668.lib(drv_uart.o)
    0x00014c2c   0x00014c2c   0x000000ce   Code   RO         2601    i.drv_uart_init     CVWL668.lib(drv_uart.o)
    0x00014cfa   0x00014cfa   0x00000002   PAD
    0x00014cfc   0x00014cfc   0x0000003c   Code   RO         2602    i.drv_uart_int_trans_handle  CVWL668.lib(drv_uart.o)
    0x00014d38   0x00014d38   0x0000001c   Code   RO         2605    i.drv_uart_reset_rx_fifo  CVWL668.lib(drv_uart.o)
    0x00014d54   0x00014d54   0x0000001c   Code   RO         2606    i.drv_uart_reset_tx_fifo  CVWL668.lib(drv_uart.o)
    0x00014d70   0x00014d70   0x0000001a   Code   RO         2607    i.drv_uart_send_blocking  CVWL668.lib(drv_uart.o)
    0x00014d8a   0x00014d8a   0x00000054   Code   RO         2609    i.drv_uart_set_baud_rate  CVWL668.lib(drv_uart.o)
    0x00014dde   0x00014dde   0x00000002   PAD
    0x00014de0   0x00014de0   0x0000004c   Code   RO         2610    i.drv_uart_trans_create_handle  CVWL668.lib(drv_uart.o)
    0x00014e2c   0x00014e2c   0x00000010   Code   RO         2508    i.drv_vidc_clear_irq  CVWL668.lib(drv_vidc.o)
    0x00014e3c   0x00014e3c   0x00000020   Code   RO         2512    i.drv_vidc_enable   CVWL668.lib(drv_vidc.o)
    0x00014e5c   0x00014e5c   0x00000040   Code   RO         2513    i.drv_vidc_enable_irq  CVWL668.lib(drv_vidc.o)
    0x00014e9c   0x00014e9c   0x0000002c   Code   RO         2514    i.drv_vidc_get_int_source  CVWL668.lib(drv_vidc.o)
    0x00014ec8   0x00014ec8   0x00000018   Code   RO         2515    i.drv_vidc_get_irq_status  CVWL668.lib(drv_vidc.o)
    0x00014ee0   0x00014ee0   0x0000002c   Code   RO         2519    i.drv_vidc_init_module_enable  CVWL668.lib(drv_vidc.o)
    0x00014f0c   0x00014f0c   0x0000000c   Code   RO         2520    i.drv_vidc_register_callback  CVWL668.lib(drv_vidc.o)
    0x00014f18   0x00014f18   0x0000000c   Code   RO         2521    i.drv_vidc_reset    CVWL668.lib(drv_vidc.o)
    0x00014f24   0x00014f24   0x0000001c   Code   RO         2522    i.drv_vidc_set_circ_mode_enable  CVWL668.lib(drv_vidc.o)
    0x00014f40   0x00014f40   0x00000038   Code   RO         2523    i.drv_vidc_set_dither_config  CVWL668.lib(drv_vidc.o)
    0x00014f78   0x00014f78   0x0000005c   Code   RO         2525    i.drv_vidc_set_dst_parameter  CVWL668.lib(drv_vidc.o)
    0x00014fd4   0x00014fd4   0x0000000c   Code   RO         2527    i.drv_vidc_set_honly_hcoef0  CVWL668.lib(drv_vidc.o)
    0x00014fe0   0x00014fe0   0x0000002c   Code   RO         2528    i.drv_vidc_set_honly_hinitb  CVWL668.lib(drv_vidc.o)
    0x0001500c   0x0001500c   0x00000030   Code   RO         2529    i.drv_vidc_set_honly_hinitr  CVWL668.lib(drv_vidc.o)
    0x0001503c   0x0001503c   0x0000001c   Code   RO         2532    i.drv_vidc_set_irqen  CVWL668.lib(drv_vidc.o)
    0x00015058   0x00015058   0x00000014   Code   RO         2533    i.drv_vidc_set_mirror  CVWL668.lib(drv_vidc.o)
    0x0001506c   0x0001506c   0x0000001c   Code   RO         2536    i.drv_vidc_set_pentile_swap  CVWL668.lib(drv_vidc.o)
    0x00015088   0x00015088   0x0000000c   Code   RO         2537    i.drv_vidc_set_pu_ctrl  CVWL668.lib(drv_vidc.o)
    0x00015094   0x00015094   0x00000018   Code   RO         2538    i.drv_vidc_set_rotation  CVWL668.lib(drv_vidc.o)
    0x000150ac   0x000150ac   0x0000000c   Code   RO         2539    i.drv_vidc_set_scld_hcoef0  CVWL668.lib(drv_vidc.o)
    0x000150b8   0x000150b8   0x0000000c   Code   RO         2540    i.drv_vidc_set_scld_hcoef1  CVWL668.lib(drv_vidc.o)
    0x000150c4   0x000150c4   0x00000014   Code   RO         2541    i.drv_vidc_set_scld_step  CVWL668.lib(drv_vidc.o)
    0x000150d8   0x000150d8   0x0000000c   Code   RO         2542    i.drv_vidc_set_scld_vcoef0  CVWL668.lib(drv_vidc.o)
    0x000150e4   0x000150e4   0x0000000c   Code   RO         2543    i.drv_vidc_set_scld_vcoef1  CVWL668.lib(drv_vidc.o)
    0x000150f0   0x000150f0   0x00000020   Code   RO         2544    i.drv_vidc_set_src_parameter  CVWL668.lib(drv_vidc.o)
    0x00015110   0x00015110   0x00000038   Code   RO         2545    i.drv_vidc_set_vintp_config  CVWL668.lib(drv_vidc.o)
    0x00015148   0x00015148   0x00000010   Code   RO         1920    i.drv_wdg_clear_counter  CVWL668.lib(drv_wdg.o)
    0x00015158   0x00015158   0x00000010   Code   RO         1921    i.drv_wdg_clear_edge_flag  CVWL668.lib(drv_wdg.o)
    0x00015168   0x00015168   0x00000010   Code   RO         1924    i.drv_wdg_read_edge_flag  CVWL668.lib(drv_wdg.o)
    0x00015178   0x00015178   0x00000034   Code   RO         1927    i.drv_wdg_set_int   CVWL668.lib(drv_wdg.o)
    0x000151ac   0x000151ac   0x00000034   Code   RO         1320    i.fputc             CVWL668.lib(tau_log.o)
    0x000151e0   0x000151e0   0x00000040   Code   RO         1464    i.ha_intl_fb_check_pu_size  CVWL668.lib(hal_internal_fb.o)
    0x00015220   0x00015220   0x00000040   Code   RO          887    i.hal_dsi_rx_ctrl_create_handle  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015260   0x00015260   0x00000040   Code   RO          888    i.hal_dsi_rx_ctrl_dcs_async_handler  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x000152a0   0x000152a0   0x00000094   Code   RO          889    i.hal_dsi_rx_ctrl_deinit  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015334   0x00015334   0x000000ac   Code   RO          895    i.hal_dsi_rx_ctrl_init  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x000153e0   0x000153e0   0x00000100   Code   RO          896    i.hal_dsi_rx_ctrl_init_clk  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x000154e0   0x000154e0   0x000000f8   Code   RO          897    i.hal_dsi_rx_ctrl_init_dsi_rx  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x000155d8   0x000155d8   0x0000012c   Code   RO          898    i.hal_dsi_rx_ctrl_init_memc  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015704   0x00015704   0x00000148   Code   RO          899    i.hal_dsi_rx_ctrl_init_rxbr  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x0001584c   0x0001584c   0x00000280   Code   RO          900    i.hal_dsi_rx_ctrl_init_vidc  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015acc   0x00015acc   0x00000038   Code   RO          901    i.hal_dsi_rx_ctrl_pre_init_pps  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015b04   0x00015b04   0x000000b0   Code   RO          907    i.hal_dsi_rx_ctrl_set_auto_ack  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015bb4   0x00015bb4   0x00000030   Code   RO          912    i.hal_dsi_rx_ctrl_set_ipi_cfg  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015be4   0x00015be4   0x00000030   Code   RO          917    i.hal_dsi_rx_ctrl_start  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015c14   0x00015c14   0x00000030   Code   RO          918    i.hal_dsi_rx_ctrl_stop  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015c44   0x00015c44   0x00000020   Code   RO          920    i.hal_dsi_rx_ctrl_toggle_resolution  CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x00015c64   0x00015c64   0x0000027c   Code   RO          967    i.hal_dsi_tx_cmd_mode_cal_timing  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00015ee0   0x00015ee0   0x00000038   Code   RO          969    i.hal_dsi_tx_ctrl_create_handle  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00015f18   0x00015f18   0x00000074   Code   RO          970    i.hal_dsi_tx_ctrl_deinit  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00015f8c   0x00015f8c   0x00000022   Code   RO          973    i.hal_dsi_tx_ctrl_gen_a_tear_signal  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00015fae   0x00015fae   0x00000002   PAD
    0x00015fb0   0x00015fb0   0x0000007c   Code   RO          975    i.hal_dsi_tx_ctrl_init  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x0001602c   0x0001602c   0x00000010   Code   RO          976    i.hal_dsi_tx_ctrl_init_clk  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x0001603c   0x0001603c   0x00000008   Code   RO          989    i.hal_dsi_tx_ctrl_set_overwrite_rgb  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00016044   0x00016044   0x0000000a   Code   RO          990    i.hal_dsi_tx_ctrl_set_tear_mode  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x0001604e   0x0001604e   0x00000002   PAD
    0x00016050   0x00016050   0x00000090   Code   RO          992    i.hal_dsi_tx_ctrl_start  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000160e0   0x000160e0   0x00000038   Code   RO          993    i.hal_dsi_tx_ctrl_stop  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00016118   0x00016118   0x000000f4   Code   RO          995    i.hal_dsi_tx_ctrl_write_array_cmd  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x0001620c   0x0001620c   0x000000d0   Code   RO          996    i.hal_dsi_tx_ctrl_write_cmd  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000162dc   0x000162dc   0x00000104   Code   RO          997    i.hal_dsi_tx_init_cfg  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000163e0   0x000163e0   0x00000038   Code   RO          998    i.hal_dsi_tx_init_dpi_timing  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00016418   0x00016418   0x00000016   Code   RO          999    i.hal_dsi_tx_init_phy_cfg  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x0001642e   0x0001642e   0x00000052   Code   RO         1000    i.hal_dsi_tx_init_timing  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00016480   0x00016480   0x00000054   Code   RO         1001    i.hal_dsi_tx_init_vid_timing  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000164d4   0x000164d4   0x00000040   Code   RO         1002    i.hal_dsi_tx_send_cmd  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00016514   0x00016514   0x00000094   Code   RO         1003    i.hal_dsi_tx_timing_info_update  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000165a8   0x000165a8   0x00000310   Code   RO         1004    i.hal_dsi_tx_vid_mode_cal_timing  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000168b8   0x000168b8   0x0000003a   Code   RO         1074    i.hal_gpio_config_pad  CVWL668.lib(hal_gpio.o)
    0x000168f2   0x000168f2   0x00000002   PAD
    0x000168f4   0x000168f4   0x00000018   Code   RO         1075    i.hal_gpio_ctrl_eint  CVWL668.lib(hal_gpio.o)
    0x0001690c   0x0001690c   0x00000040   Code   RO         1079    i.hal_gpio_init_eint  CVWL668.lib(hal_gpio.o)
    0x0001694c   0x0001694c   0x00000016   Code   RO         1080    i.hal_gpio_init_input  CVWL668.lib(hal_gpio.o)
    0x00016962   0x00016962   0x0000001c   Code   RO         1081    i.hal_gpio_init_output  CVWL668.lib(hal_gpio.o)
    0x0001697e   0x0001697e   0x00000002   PAD
    0x00016980   0x00016980   0x0000001c   Code   RO         1082    i.hal_gpio_reg_eint_cb  CVWL668.lib(hal_gpio.o)
    0x0001699c   0x0001699c   0x00000050   Code   RO         1083    i.hal_gpio_set_ap_reset_int  CVWL668.lib(hal_gpio.o)
    0x000169ec   0x000169ec   0x00000060   Code   RO         1086    i.hal_gpio_set_mode  CVWL668.lib(hal_gpio.o)
    0x00016a4c   0x00016a4c   0x00000008   Code   RO         1087    i.hal_gpio_set_output_data  CVWL668.lib(hal_gpio.o)
    0x00016a54   0x00016a54   0x00000010   Code   RO         1372    i.hal_internal_sync_get_hight_performan_mode  CVWL668.lib(hal_internal_vsync.o)
    0x00016a64   0x00016a64   0x000001ac   Code   RO         1373    i.hal_internal_sync_input_resolution_change  CVWL668.lib(hal_internal_vsync.o)
    0x00016c10   0x00016c10   0x0000000c   Code   RO         1374    i.hal_internal_sync_register_lcdc_cb  CVWL668.lib(hal_internal_vsync.o)
    0x00016c1c   0x00016c1c   0x00000020   Code   RO         1377    i.hal_internal_vsync_deinit  CVWL668.lib(hal_internal_vsync.o)
    0x00016c3c   0x00016c3c   0x0000000c   Code   RO         1378    i.hal_internal_vsync_get_rx_state  CVWL668.lib(hal_internal_vsync.o)
    0x00016c48   0x00016c48   0x00000014   Code   RO         1379    i.hal_internal_vsync_get_sync_line  CVWL668.lib(hal_internal_vsync.o)
    0x00016c5c   0x00016c5c   0x0000000c   Code   RO         1380    i.hal_internal_vsync_get_tx_state  CVWL668.lib(hal_internal_vsync.o)
    0x00016c68   0x00016c68   0x000000e8   Code   RO         1381    i.hal_internal_vsync_init_rx  CVWL668.lib(hal_internal_vsync.o)
    0x00016d50   0x00016d50   0x000000c8   Code   RO         1382    i.hal_internal_vsync_init_tx  CVWL668.lib(hal_internal_vsync.o)
    0x00016e18   0x00016e18   0x00000020   Code   RO         1383    i.hal_internal_vsync_set_rx_state  CVWL668.lib(hal_internal_vsync.o)
    0x00016e38   0x00016e38   0x00000144   Code   RO         1385    i.hal_internal_vsync_set_tear_mode  CVWL668.lib(hal_internal_vsync.o)
    0x00016f7c   0x00016f7c   0x00000058   Code   RO         1386    i.hal_internal_vsync_set_tx_state  CVWL668.lib(hal_internal_vsync.o)
    0x00016fd4   0x00016fd4   0x0000006c   Code   RO         1437    i.hal_intl_dcs_init_sw_fltr  CVWL668.lib(hal_internal_dcs.o)
    0x00017040   0x00017040   0x0000044c   Code   RO         1439    i.hal_intl_dcs_rx_get_dcs_packet_data  CVWL668.lib(hal_internal_dcs.o)
    0x0001748c   0x0001748c   0x00000088   Code   RO         1440    i.hal_intl_dcs_rx_receive_packet  CVWL668.lib(hal_internal_dcs.o)
    0x00017514   0x00017514   0x00000174   Code   RO         1441    i.hal_intl_dcs_rx_receive_pps  CVWL668.lib(hal_internal_dcs.o)
    0x00017688   0x00017688   0x0000008c   Code   RO         1442    i.hal_intl_dcs_set_auto_hw_filter  CVWL668.lib(hal_internal_dcs.o)
    0x00017714   0x00017714   0x0000002c   Code   RO         1444    i.hal_intl_dcs_sw_filter_handle  CVWL668.lib(hal_internal_dcs.o)
    0x00017740   0x00017740   0x000002f0   Code   RO         1465    i.hal_intl_fb_cal_fb_info  CVWL668.lib(hal_internal_fb.o)
    0x00017a30   0x00017a30   0x00000064   Code   RO         1466    i.hal_intl_fb_check_bandwidth  CVWL668.lib(hal_internal_fb.o)
    0x00017a94   0x00017a94   0x000000dc   Code   RO         1467    i.hal_intl_fb_edge_resize  CVWL668.lib(hal_internal_fb.o)
    0x00017b70   0x00017b70   0x00000074   Code   RO         1468    i.hal_intl_fb_flow_control_adapter  CVWL668.lib(hal_internal_fb.o)
    0x00017be4   0x00017be4   0x0000000c   Code   RO         1469    i.hal_intl_fb_get_memc_flow_mode  CVWL668.lib(hal_internal_fb.o)
    0x00017bf0   0x00017bf0   0x00000010   Code   RO         1470    i.hal_intl_fb_get_rx_fb_info  CVWL668.lib(hal_internal_fb.o)
    0x00017c00   0x00017c00   0x00000010   Code   RO         1471    i.hal_intl_fb_get_tx_fb_info  CVWL668.lib(hal_internal_fb.o)
    0x00017c10   0x00017c10   0x0000000c   Code   RO         1472    i.hal_intl_fb_get_user_flow  CVWL668.lib(hal_internal_fb.o)
    0x00017c1c   0x00017c1c   0x00000028   Code   RO         1490    i.hal_intl_svs_deinit_rx  CVWL668.lib(hal_internal_svs.o)
    0x00017c44   0x00017c44   0x00000010   Code   RO         1491    i.hal_intl_svs_deinit_tx  CVWL668.lib(hal_internal_svs.o)
    0x00017c54   0x00017c54   0x00000024   Code   RO         1492    i.hal_intl_svs_handle  CVWL668.lib(hal_internal_svs.o)
    0x00017c78   0x00017c78   0x00000080   Code   RO         1493    i.hal_intl_svs_init_rx  CVWL668.lib(hal_internal_svs.o)
    0x00017cf8   0x00017cf8   0x00000014   Code   RO         1494    i.hal_intl_svs_init_tx  CVWL668.lib(hal_internal_svs.o)
    0x00017d0c   0x00017d0c   0x0000000c   Code   RO         1496    i.hal_intl_svs_set_rx_vtt  CVWL668.lib(hal_internal_svs.o)
    0x00017d18   0x00017d18   0x00000048   Code   RO         1498    i.hal_intl_svs_update_rxbr_clk  CVWL668.lib(hal_internal_svs.o)
    0x00017d60   0x00017d60   0x00000070   Code   RO         1005    i.hal_lcdc_displayproc_config  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00017dd0   0x00017dd0   0x0000003e   Code   RO         1006    i.hal_lcdc_init_cfg  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00017e0e   0x00017e0e   0x00000070   Code   RO         1007    i.hal_lcdc_init_clk  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00017e7e   0x00017e7e   0x00000002   PAD
    0x00017e80   0x00017e80   0x00000128   Code   RO         1008    i.hal_lcdc_postproc_config  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00017fa8   0x00017fa8   0x00000024   Code   RO         1009    i.hal_lcdc_start    CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00017fcc   0x00017fcc   0x0000003c   Code   RO         1010    i.hal_lcdc_timinggen_config  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00018008   0x00018008   0x000000e0   Code   RO         1011    i.hal_lcdc_upscaler_config  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000180e8   0x000180e8   0x000000bc   Code   RO         1013    i.hal_nonshadow_func_update  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000181a4   0x000181a4   0x0000002a   Code   RO         1271    i.hal_pwr_enter_deep_sleep_mode  CVWL668.lib(hal_pwr.o)
    0x000181ce   0x000181ce   0x00000008   Code   RO         1272    i.hal_pwr_enter_normal_sleep_mode  CVWL668.lib(hal_pwr.o)
    0x000181d6   0x000181d6   0x00000002   PAD
    0x000181d8   0x000181d8   0x00000064   Code   RO         1273    i.hal_pwr_enter_stop_sleep_mode  CVWL668.lib(hal_pwr.o)
    0x0001823c   0x0001823c   0x0000000a   Code   RO         1274    i.hal_pwr_exit_sleep_mode  CVWL668.lib(hal_pwr.o)
    0x00018246   0x00018246   0x00000008   Code   RO         1276    i.hal_pwr_get_vcc_power_ready  CVWL668.lib(hal_pwr.o)
    0x0001824e   0x0001824e   0x00000008   Code   RO         1281    i.hal_pwr_set_main_power  CVWL668.lib(hal_pwr.o)
    0x00018256   0x00018256   0x00000008   Code   RO         1283    i.hal_pwr_set_sleep_mode_power  CVWL668.lib(hal_pwr.o)
    0x0001825e   0x0001825e   0x00000002   PAD
    0x00018260   0x00018260   0x00000064   Code   RO         1284    i.hal_pwr_set_stop_sleep_wakeup_pin  CVWL668.lib(hal_pwr.o)
    0x000182c4   0x000182c4   0x00000040   Code   RO         1168    i.hal_swire_deinit  CVWL668.lib(hal_swire.o)
    0x00018304   0x00018304   0x0000005c   Code   RO         1169    i.hal_swire_enable  CVWL668.lib(hal_swire.o)
    0x00018360   0x00018360   0x00000058   Code   RO         1170    i.hal_swire_init    CVWL668.lib(hal_swire.o)
    0x000183b8   0x000183b8   0x00000024   Code   RO         1172    i.hal_swire_set_pulse  CVWL668.lib(hal_swire.o)
    0x000183dc   0x000183dc   0x00000040   Code   RO         1173    i.hal_swire_set_timer  CVWL668.lib(hal_swire.o)
    0x0001841c   0x0001841c   0x000000e4   Code   RO         1193    i.hal_system_init   CVWL668.lib(hal_system.o)
    0x00018500   0x00018500   0x00000050   Code   RO         1196    i.hal_system_updata_sysclk  CVWL668.lib(hal_system.o)
    0x00018550   0x00018550   0x00000030   Code   RO         1211    i.hal_timer_deinit  CVWL668.lib(hal_timer.o)
    0x00018580   0x00018580   0x0000001c   Code   RO         1213    i.hal_timer_init    CVWL668.lib(hal_timer.o)
    0x0001859c   0x0001859c   0x00000008   Code   RO         1214    i.hal_timer_set_repeat  CVWL668.lib(hal_timer.o)
    0x000185a4   0x000185a4   0x00000030   Code   RO         1215    i.hal_timer_start   CVWL668.lib(hal_timer.o)
    0x000185d4   0x000185d4   0x00000028   Code   RO         1217    i.hal_timer_stop    CVWL668.lib(hal_timer.o)
    0x000185fc   0x000185fc   0x00000030   Code   RO         1014    i.hal_tx_frame_rate_adjust  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x0001862c   0x0001862c   0x00000094   Code   RO         1344    i.hal_uart_init     CVWL668.lib(hal_uart.o)
    0x000186c0   0x000186c0   0x0000001c   Code   RO         1347    i.hal_uart_send_blocking  CVWL668.lib(hal_uart.o)
    0x000186dc   0x000186dc   0x00000018   Code   RO         1015    i.hal_vsync_func_update  CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x000186f4   0x000186f4   0x000000e0   Code   RO         1388    i.hal_vsync_reset_lcdc_scaler  CVWL668.lib(hal_internal_vsync.o)
    0x000187d4   0x000187d4   0x00000040   Code   RO            3    i.main              main.o
    0x00018814   0x00018814   0x00000054   Code   RO          344    i.pps_update_handle  s8_demo.o
    0x00018868   0x00018868   0x000002e4   Code   RO         1389    i.rxbr_irq1_callback  CVWL668.lib(hal_internal_vsync.o)
    0x00018b4c   0x00018b4c   0x00000060   Code   RO          345    i.s8_demo           s8_demo.o
    0x00018bac   0x00018bac   0x0000003a   Code   RO          346    i.send_panel_init_code  s8_demo.o
    0x00018be6   0x00018be6   0x00000002   PAD
    0x00018be8   0x00018be8   0x00000044   Code   RO         1390    i.soft_double_buffer_update  CVWL668.lib(hal_internal_vsync.o)
    0x00018c2c   0x00018c2c   0x0000006c   Code   RO         1391    i.soft_gen_te       CVWL668.lib(hal_internal_vsync.o)
    0x00018c98   0x00018c98   0x000000e0   Code   RO         1392    i.soft_gen_te_double_buffer  CVWL668.lib(hal_internal_vsync.o)
    0x00018d78   0x00018d78   0x00000038   Code   RO         1393    i.soft_pro_motion_init  CVWL668.lib(hal_internal_vsync.o)
    0x00018db0   0x00018db0   0x00000038   Code   RO          347    i.soft_swire_init   s8_demo.o
    0x00018de8   0x00018de8   0x0000002e   Code   RO          348    i.soft_swire_start  s8_demo.o
    0x00018e16   0x00018e16   0x00000002   PAD
    0x00018e18   0x00018e18   0x00000048   Code   RO          349    i.soft_swire_timer_callback  s8_demo.o
    0x00018e60   0x00018e60   0x00000024   Code   RO         1394    i.soft_tear_adjust_line  CVWL668.lib(hal_internal_vsync.o)
    0x00018e84   0x00018e84   0x00000018   Code   RO         1286    i.stop_sleep_cb     CVWL668.lib(hal_pwr.o)
    0x00018e9c   0x00018e9c   0x000000ac   Code   RO         1499    i.svs_direct_mode_setting  CVWL668.lib(hal_internal_svs.o)
    0x00018f48   0x00018f48   0x0000001c   Code   RO         1500    i.svs_get_rel_intv  CVWL668.lib(hal_internal_svs.o)
    0x00018f64   0x00018f64   0x000000b0   Code   RO         1501    i.svs_sync_handle   CVWL668.lib(hal_internal_svs.o)
    0x00019014   0x00019014   0x000000cc   Code   RO         1502    i.svs_wait_fr_stab  CVWL668.lib(hal_internal_svs.o)
    0x000190e0   0x000190e0   0x0000010c   Code   RO         1503    i.svs_wait_start    CVWL668.lib(hal_internal_svs.o)
    0x000191ec   0x000191ec   0x00000034   Code   RO         1321    i.tau_log_init      CVWL668.lib(tau_log.o)
    0x00019220   0x00019220   0x00000084   Code   RO         1322    i.tau_log_printf    CVWL668.lib(tau_log.o)
    0x000192a4   0x000192a4   0x00000076   Code   RO         1323    i.tau_log_push_log  CVWL668.lib(tau_log.o)
    0x0001931a   0x0001931a   0x00000002   PAD
    0x0001931c   0x0001931c   0x000000b4   Code   RO         1395    i.vidc_callback     CVWL668.lib(hal_internal_vsync.o)
    0x000193d0   0x000193d0   0x00000118   Code   RO         1396    i.vpre_err_reset    CVWL668.lib(hal_internal_vsync.o)
    0x000194e8   0x000194e8   0x00001efc   Data   RO          350    .constdata          s8_demo.o
    0x0001b3e4   0x0001b3e4   0x00000028   Data   RO          922    .constdata          CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x0001b40c   0x0001b40c   0x0000001c   Data   RO         1018    .constdata          CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x0001b428   0x0001b428   0x000000b6   Data   RO         1091    .constdata          CVWL668.lib(hal_gpio.o)
    0x0001b4de   0x0001b4de   0x00000002   PAD
    0x0001b4e0   0x0001b4e0   0x00000030   Data   RO         1349    .constdata          CVWL668.lib(hal_uart.o)
    0x0001b510   0x0001b510   0x00000010   Data   RO         2612    .constdata          CVWL668.lib(drv_uart.o)
    0x0001b520   0x0001b520   0x00000087   Data   RO          923    .conststring        CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x0001b5a7   0x0001b5a7   0x00000001   PAD
    0x0001b5a8   0x0001b5a8   0x00000090   Data   RO         1398    .conststring        CVWL668.lib(hal_internal_vsync.o)
    0x0001b638   0x0001b638   0x0000008e   Data   RO         1447    .conststring        CVWL668.lib(hal_internal_dcs.o)
    0x0001b6c6   0x0001b6c6   0x00000002   PAD
    0x0001b6c8   0x0001b6c8   0x00000020   Data   RO         3012    Region$$Table       anon$$obj.o


    Execution Region RW_IRAM1 (Exec base: 0x00070000, Load base: 0x0001b6e8, Size: 0x00003120, Max: 0x00008000, ABSOLUTE, COMPRESSED[0x00000160])

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00070000   COMPRESSED   0x0000008f   Data   RW          351    .data               s8_demo.o
    0x0007008f   COMPRESSED   0x00000001   PAD
    0x00070090   COMPRESSED   0x00000024   Data   RW          924    .data               CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x000700b4   COMPRESSED   0x0000005c   Data   RW         1019    .data               CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00070110   COMPRESSED   0x00000001   Data   RW         1154    .data               CVWL668.lib(hal_spi_master.o)
    0x00070111   COMPRESSED   0x00000002   Data   RW         1175    .data               CVWL668.lib(hal_swire.o)
    0x00070113   COMPRESSED   0x00000001   PAD
    0x00070114   COMPRESSED   0x00000008   Data   RW         1287    .data               CVWL668.lib(hal_pwr.o)
    0x0007011c   COMPRESSED   0x00000001   Data   RW         1326    .data               CVWL668.lib(tau_log.o)
    0x0007011d   COMPRESSED   0x00000003   PAD
    0x00070120   COMPRESSED   0x00000018   Data   RW         1350    .data               CVWL668.lib(hal_uart.o)
    0x00070138   COMPRESSED   0x00000010   Data   RW         1399    .data               CVWL668.lib(hal_internal_vsync.o)
    0x00070148   COMPRESSED   0x00000024   Data   RW         1448    .data               CVWL668.lib(hal_internal_dcs.o)
    0x0007016c   COMPRESSED   0x0000000c   Data   RW         1532    .data               CVWL668.lib(drv_common.o)
    0x00070178   COMPRESSED   0x00000001   Data   RW         1533    .data               CVWL668.lib(drv_common.o)
    0x00070179   COMPRESSED   0x00000003   PAD
    0x0007017c   COMPRESSED   0x00000190   Data   RW         1618    .data               CVWL668.lib(drv_dma.o)
    0x0007030c   COMPRESSED   0x00000004   Data   RW         1682    .data               CVWL668.lib(drv_gpio.o)
    0x00070310   COMPRESSED   0x00000004   Data   RW         1852    .data               CVWL668.lib(drv_swire.o)
    0x00070314   COMPRESSED   0x00000050   Data   RW         1900    .data               CVWL668.lib(drv_timer.o)
    0x00070364   COMPRESSED   0x0000000c   Data   RW         1929    .data               CVWL668.lib(drv_wdg.o)
    0x00070370   COMPRESSED   0x00000024   Data   RW         2016    .data               CVWL668.lib(drv_i2c.o)
    0x00070394   COMPRESSED   0x00000004   Data   RW         2085    .data               CVWL668.lib(drv_se.o)
    0x00070398   COMPRESSED   0x00000001   Data   RW         2125    .data               CVWL668.lib(drv_dsi_rx.o)
    0x00070399   COMPRESSED   0x00000003   PAD
    0x0007039c   COMPRESSED   0x00000008   Data   RW         2460    .data               CVWL668.lib(drv_rxbr.o)
    0x000703a4   COMPRESSED   0x00000004   Data   RW         2547    .data               CVWL668.lib(drv_vidc.o)
    0x000703a8   COMPRESSED   0x00000004   Data   RW         2990    .data               mc_p.l(stdout.o)
    0x000703ac        -       0x000000d0   Zero   RW          921    .bss                CVWL668.lib(hal_dsi_rx_ctrl.o)
    0x0007047c        -       0x000000b8   Zero   RW         1017    .bss                CVWL668.lib(hal_dsi_tx_ctrl.o)
    0x00070534        -       0x00000100   Zero   RW         1325    .bss                CVWL668.lib(tau_log.o)
    0x00070634        -       0x00000044   Zero   RW         1397    .bss                CVWL668.lib(hal_internal_vsync.o)
    0x00070678        -       0x00000800   Zero   RW         1445    .bss                CVWL668.lib(hal_internal_dcs.o)
    0x00070e78        -       0x000000ff   Zero   RW         1446    .bss                CVWL668.lib(hal_internal_dcs.o)
    0x00070f77   COMPRESSED   0x00000001   PAD
    0x00070f78        -       0x00000044   Zero   RW         1474    .bss                CVWL668.lib(hal_internal_fb.o)
    0x00070fbc        -       0x00000044   Zero   RW         1504    .bss                CVWL668.lib(hal_internal_svs.o)
    0x00071000        -       0x00000010   Zero   RW         1616    .bss                CVWL668.lib(drv_dma.o)
    0x00071010        -       0x00000040   Zero   RW         1681    .bss                CVWL668.lib(drv_gpio.o)
    0x00071050        -       0x0000106c   Zero   RW         2068    .bss                CVWL668.lib(dcs_packet_fifo.o)
    0x000720bc        -       0x00000060   Zero   RW         2611    .bss                CVWL668.lib(drv_uart.o)
    0x0007211c   COMPRESSED   0x00000004   PAD
    0x00072120        -       0x00001000   Zero   RW          536    STACK               startup_armcm0.o


==============================================================================

Image component sizes


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Object Name

         0          0          0          0          0       5336   app_tp_transfer.o
        24          4          0          0          0        581   board.o
        64         32          0          0          0      10483   main.o
      2544        602       7932        143          0      26845   s8_demo.o
       120         18        192          0       4096       2148   startup_armcm0.o

    ----------------------------------------------------------------------
      2760        656       8156        144       4096      45393   Object Totals
         0          0         32          0          0          0   (incl. Generated)
         8          0          0          1          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Member Name

       216         32          0          0       4204        252   dcs_packet_fifo.o
       104         62         28         13          0        192   drv_common.o
       536         90          0          0          0        792   drv_crgu.o
       136         22          0        400         16        196   drv_dma.o
       144         34          0          0          0        248   drv_dsc_dec.o
      1892        678          0          1          0       1280   drv_dsi_rx.o
      1704        306          0          0          0       2036   drv_dsi_tx.o
       148          0          0          0          0        260   drv_efuse.o
       296         40          0          4         64       1000   drv_gpio.o
        36         12          0         36          0        180   drv_i2c.o
      1080        166          0          0          0       1620   drv_lcdc.o
       658        104          0          0          0       1240   drv_memc.o
        40          0          0          0          0        120   drv_phy_common.o
       592        132          0          0          0        716   drv_pwr.o
       814        110          0          8          0       1136   drv_rxbr.o
      1012        264          0          4          0        492   drv_se.o
        88         20          0          0          0        188   drv_spi_master.o
       264         54          0          4          0        560   drv_swire.o
       220         40          0          0          0        428   drv_sys_cfg.o
       386         44          0         80          0        876   drv_timer.o
      1172         54         16          0         96        980   drv_uart.o
       824        152          0          4          0       1700   drv_vidc.o
       156         22          0         12          0        316   drv_wdg.o
      2654        196        175         36        208       1168   hal_dsi_rx_ctrl.o
      4314        338         50         92        184       2212   hal_dsi_tx_ctrl.o
       440         32        182          0          0        688   hal_gpio.o
      2168        508        142         36       2303        652   hal_internal_dcs.o
      1308         60          0          0         68        700   hal_internal_fb.o
      1172        182          0          0         68        840   hal_internal_svs.o
      3648        756        144         16         68       1688   hal_internal_vsync.o
       308         32          0          8          0        616   hal_pwr.o
        72         10          0          1          0         68   hal_spi_master.o
       344         32          0          2          0        348   hal_swire.o
       308         56          0          0          0        136   hal_system.o
       172          0          0          0          0        344   hal_timer.o
       176         18         48         24          0        144   hal_uart.o
        68          4          0          0          0        136   tau_delay.o
       354         30         16          1        256        320   tau_log.o
       200         20          0          0          0         76   ceil.o
        86          0          0          0          0          0   __dczerorl2.o
         0          0          0          0          0          0   entry.o
         0          0          0          0          0          0   entry10a.o
         0          0          0          0          0          0   entry11a.o
         8          4          0          0          0          0   entry2.o
         4          0          0          0          0          0   entry5.o
         0          0          0          0          0          0   entry7b.o
         0          0          0          0          0          0   entry8b.o
         8          4          0          0          0          0   entry9a.o
        30          0          0          0          0          0   handlers.o
        40          0          0          0          0         72   idiv.o
        36          8          0          0          0         68   init.o
         0          0          0          0          0          0   iusefp.o
        32          0          0          0          0         68   llshl.o
        38          0          0          0          0         68   llsshr.o
        34          0          0          0          0         68   llushr.o
        36          0          0          0          0         60   memcpya.o
        36          0          0          0          0        100   memseta.o
      2298        104          0          0          0        544   printfa.o
         0          0          0          4          0          0   stdout.o
        14          0          0          0          0         60   strlen.o
        44          0          0          0          0         72   uidiv.o
        96          0          0          0          0         84   uldiv.o
        40          2          0          0          0         68   cdrcmple.o
        20          0          0          0          0         68   cfcmple.o
        20          0          0          0          0         68   cfrcmple.o
        56          0          0          0          0         68   d2f.o
       356          4          0          0          0        140   dadd.o
       240          6          0          0          0         84   ddiv.o
       236          0          0          0          0        216   depilogue.o
        60         10          0          0          0         68   dfixui.o
        64         10          0          0          0         68   dfixul.o
        28          4          0          0          0         68   dfltui.o
       208          6          0          0          0         88   dmul.o
        40          0          0          0          0         60   f2d.o
       178          0          0          0          0        108   fadd.o
       124          0          0          0          0         72   fdiv.o
       130          0          0          0          0        144   fepilogue.o
        40          0          0          0          0         60   ffixui.o
        14          0          0          0          0         68   ffltui.o
       122          0          0          0          0         72   fmul.o
        24          0          0          0          0         60   fscalb.o

    ----------------------------------------------------------------------
     35100       4874        808        796       7540      29856   Library Totals
        36          0          7         10          5          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Name

     30024       4692        801        782       7535      26868   CVWL668.lib
       200         20          0          0          0         76   m_ps.l
      2840        120          0          4          0       1264   mc_p.l
      2000         42          0          0          0       1648   mf_p.l

    ----------------------------------------------------------------------
     35100       4874        808        796       7540      29856   Library Totals

    ----------------------------------------------------------------------

==============================================================================


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   

     37860       5530       8964        940      11636      55165   Grand Totals
     37860       5530       8964        352      11636      55165   ELF Image Totals (compressed)
     37860       5530       8964        352          0          0   ROM Totals

==============================================================================

    Total RO  Size (Code + RO Data)                46824 (  45.73kB)
    Total RW  Size (RW Data + ZI Data)             12576 (  12.28kB)
    Total ROM Size (Code + RO Data + RW Data)      47176 (  46.07kB)

==============================================================================

